**3GPP TSG-RAN WG3 Meeting #113-e R3-214381 was R3-213556**

**E-meeting, 16-26 Aug 2021**

**Title:** (TP to TS 38.410 BL CR) Multicast Session Management

**Source:** Huawei, CBN, China Unicom, Lenovo, Motorola Mobility, Qualcomm Incorporated, China Telecom, Nokia, Nokia Shanghai Bell, CMCC

**Agenda item:** 22.2.2

**Document Type:** Other

# 1. Text Proposal to BL CR of TS 38.410

***-----------------Start of the Changes-------------------***

# 5 Functions of the NG interface

***//skip unchanged part***

5.xx NR MBS Session Management function

The MBS Session Management function is responsible for establishing, modifying and releasing the involved NR MBS sessions NG-RAN resources for user data transport once an MBS context is available in the NG-RAN node.

Editor’s Note: this only applies to broadcast.

5.yy Multicast Group Paging Function

The Multicast group paging function supports the sending of multicast group paging requests to the NG-RAN nodes in order to group-page UEs that have joined the Multicast MBS Session.

# 6 Signalling procedures of the NG interface

***//skip unchanged part***

6.xx NR MBS Session Management Procedures

The following list of MBS Session management procedures are used to establish, release, or modify NG-RAN resources for a NR MBS session:

- Broadcast Session Resource Setup;

- Broadcast Session Resource Release;

Editor’s Note: this only applies to broadcast.

6.yy Multicast Group Paging Procedures

The following Multicast Group Paging procedure is used to send multicast group paging requests to the NG-RAN nodes:

- Multicast Group Paging.

***-----------------End of the Changes-------------------***