**3GPP TSG-RAN WG3#116-e R3-22xxxx**

**E-Meeting, 09 – 19 May 2022**

**Title:** [Draft]LS on RB set configuration for IAB

**Response to:**

**Release:** Rel-17

**Work Item:** NR\_IAB\_enh-Core

**Source:** Huawei (to be RAN3)

**To:** RAN1

**Cc:**

**Contact Person:**

#### Name: Yuanping Zhu

**Tel. Number:**

E-mail Address: zhuyuanping@huawei.com

**1. Overall Description:**

RAN3 has captured the RB set configuration in F1AP and XnAP specification. The description in the current F1AP specification indicates that the RB set Configuration also applicable for the IAB-donor-DU, but companies in RAN3 do not have consensus on this issue. Consequently, RAN3 would like to ask RAN1 to clarify whether the RB set needs to be configured to the IAB-donor-DU, and inform RAN3 about the outcome.

**2. Actions:**

**To RAN1 group:**

**ACTION:** RAN3 respectfully asks RAN1 to clarify whether the RB set needs to be configured to the IAB-donor-DU.

**3. Date of Next TSG-RAN WG3 Meetings:**

TSG-RAN WG3#117-e 15 August – 25 August 2022 E-meeting