**3GPP TSG-RAN WG3 #117bis-eR3-22xxx**

**Online, 10 – 18 October 2022**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  |  | **CR** | **xxxx** | **rev** | **-** | **Current version:** |  |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **X** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | PDCP COUNT reset in CU-UP for inter-gNB-DU Handover |
|  |  |
| ***Source to WG:*** | NEC, .... |
| ***Source to TSG:*** |  |
|  |  |
| ***Work item code:*** | NR\_CPUP\_Split-Core, TEI16 |  | ***Date:*** | 2022-10-13 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** |  |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | For the inter-gNB-DU handover when *CellGroupConfig* is generated using full configuration by the target gNB-DU, while gNB-CU decide to keep the same gNB-CU-UP that need to reset the PDCP COUNT of the existing DRBs, two time of the signalling procedures is needed.i.e. the E1AP: Bearer Context Modification procedures (first to release DRBs + adding the same DRBs, second to give Target DU’s DL TNL address), this takes longer time to complete the whole hanover procedure.  |
|  |  |
| ***Summary of change:*** | New *Handover With Full Configuration* IE is added at the BEARER CONTEXT MODIFICATION REQUEST message.Adding text in procedure text. Impact Analysis:Impact assessment towards the previous version of the specification (same release): This CR has isolated impact with the previous version of the specification (same release) because the correction only related with Bearer Context Modification procedure. |
|  |  |
| ***Consequences if not approved:*** | Unable to do the PDCP COUNT reset in a single Bearer Context Modification procedure. |
|  |  |
| ***Clauses affected:*** | 8.3.2.2, 9.2.2.4, ASN.1 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** | **X** |  |  Other core specifications  | TS37.483 CR 00xx |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

<<<<<<<<<<<<<<<<<<<< Change >>>>>>>>>>>>>>>>>>>>

### 8.3.2 Bearer Context Modification (gNB-CU-CP initiated)

#### 8.3.2.1 General

The purpose of the Bearer Context Modification procedure is to allow the gNB-CU-CP to modify a bearer context in the gNB-CU-UP. The procedure uses UE-associated signalling.

#### 8.3.2.2 Successful Operation



Figure 8.3.2.2-1: Bearer Context Modification procedure: Successful Operation.

The gNB-CU-CP initiates the procedure by sending the BEARER CONTEXT MODIFICATION REQUEST message to the gNB-CU-UP. If the gNB-CU-UP succeeds to modify the bearer context, it replies to the gNB-CU-CP with the BEARER CONTEXT MODIFICATION RESPONSE message.

The gNB-CU-UP shall report to the gNB-CU-CP, in the BEARER CONTEXT MODIFICATION RESPONSE message, the result for all the requested resources in the following way:

For E-UTRAN:

- A list of DRBs which are successfully established shall be included in the *DRB Setup List* IE;

- A list of DRBs which failed to be established shall be included in the *DRB Failed List* IE;

- A list of DRBs which are successfully modified shall be included in the *DRB Modified List* IE;

- A list of DRBs which failed to be modified shall be included in the *DRB Failed To Modify List* IE;

For NG-RAN:

- A list of PDU Session Resources which are successfully established shall be included in the *PDU Session Resource Setup List* IE;

- A list of PDU Session Resources which failed to be established shall be included in the *PDU Session Resource Failed List* IE;

- A list of PDU Session Resources which are successfully modified shall be included in the *PDU Session Resource Modified List* IE;

- A list of PDU Session Resources which failed to be modified shall be included in the *PDU Session Resource Failed To Modify List* IE;

- For each successfully established or modified PDU Session Resource, a list of DRBs which are successfully established shall be included in the *DRB Setup List* IE;

- For each successfully established or modified PDU Session Resource, a list of DRBs which failed to be established shall be included in the *DRB Failed List* IE;

- For each successfully modified PDU Session Resource, a list of DRBs which are successfully modified shall be included in the *DRB Modified List* IE;

- For each successfully modified PDU Session Resource, a list of DRBs which failed to be modified shall be included in the *DRB Failed To Modify List* IE;

- For each successfully established or modified DRB, a list of QoS Flows which are successfully established shall be included in the *Flow Setup List* IE;

- For each successfully established or modified DRB, a list of QoS Flows which failed to be established shall be included in the *Flow Failed List* IE;

When the gNB-CU-UP reports the unsuccessful establishment of a PDU Session Resource, DRB or QoS Flow the cause value should be precise enough to enable the gNB-CU-CP to know the reason for the unsuccessful establishment.

If the *Security Information* IE is contained in the BEARER CONTEXT MODIFICATION REQUEST message, the gNB-CU-UP shall update the corresponding information.

If the *UE DL Aggregate Maximum Bit Rate* IE is contained in the BEARER CONTEXT MODIFICATION REQUEST message, the gNB-CU-UP shall update the corresponding information.

If the *UE DL Maximum Integrity Protected Data Rate* IE is contained in the BEARER CONTEXT MODIFICATION REQUEST message, the gNB-CU-UP shall update the corresponding information.

If the *Bearer Context Status Change* IE is contained in the BEARER CONTEXT MODIFICATION REQUEST message, the gNB-CU-UP shall consider the UE RRC state and act as specified in TS 38.401 [2].

If the *Data Forwarding Information Request* IE, *PDU Session Data Forwarding Information Request* IE or the *DRB Data Forwarding Information Request* IE are included in the BEARER CONTEXT MODIFICATION REQUEST message, the gNB-CU-UP shall include the requested forwarding information in the *Data Forwarding Information Response* IE, *PDU Session Data Forwarding Information Response* IE or the *DRB Data Forwarding Information Response* IE in the BEARER CONTEXT MODIFICATION RESPONSE message.

If the *PDU Session Data Forwarding Information* IE is included in the BEARER CONTEXT MODIFICATION REQUEST message, the gNB-CU-UP shall, if supported, consider that data forwarding is applicable for the indicated QoS flows for the concerned PDU session.

If the *PDCP Configuration* IE is contained in the *DRB To Modify List* IE in the BEARER CONTEXT MODIFICATION REQUEST message, the gNB-CU-UP shall update the corresponding information, except for the *PDCP SN UL Size* IE, the *PDCP SN DL Size* IE and the *RLC mode* IE which shall be ignored.

If the *E-UTRAN QoS* IE is contained in the *DRB To Modify List* IE in the BEARER CONTEXT MODIFICATION REQUEST message, the gNB-CU-UP shall update the corresponding information.

If the *PDCP SN Status Request* IE is contained in the *DRB To Modify List* IE in the BEARER CONTEXT MODIFICATION REQUEST message, the gNB-CU-UP shall act as specified in TS 38.401 [2] and include the *UL COUNT Value* IE and the *DL COUNT Value* IE in the BEARER CONTEXT MODIFICATION RESPONSE message.

If the *PDCP SN Status Information* IE is contained in the *DRB To Setup List* IE or the *DRB To Modify List* IE in the BEARER CONTEXT MODIFICATION REQUEST message, the gNB-CU-UP shall take it into account and act as specified in TS 38.401 [2].

If the *DL UP Parameters* IE is contained in the *DRB To Modify List* IE in the BEARER CONTEXT MODIFICATION REQUEST message, the gNB-CU-UP shall update the corresponding information.

If the *Cell Group To Add* IE or the *Cell Group To Modify* IE or the *Cell Group To Remove* IE is contained in the *DRB To Modify List* IE in the BEARER CONTEXT MODIFICATION REQUEST message, the gNB-CU-UP shall add or modify or remove the corresponding cell group.

If the *PDU Session Resource DL Aggregate Maximum Bit Rate* IE is contained in the *PDU Session Resource To Setup List* IE in the BEARER CONTEXT MODIFICATION REQUEST message, the gNB-CU-UP shall replace the information in the UE context and use it when enforcing downlink traffic policing for the non GBR QoS flows for the concerned UE, as specified in TS 23.501 [20].

If the *PDU Session Resource DL Aggregate Maximum Bit Rate* IE is contained in the *PDU Session Resource To Modify List* IE in the BEARER CONTEXT MODIFICATION REQUEST message, the gNB-CU-UP shall update the corresponding information.

If the *SDAP Configuration* IE is contained in the *DRB To Modify List* IE in the BEARER CONTEXT MODIFICATION REQUEST message, the gNB-CU-UP shall update the corresponding information.

If the *Flow Mapping Information* IE is contained in the *DRB To Modify List* IE in the BEARER CONTEXT MODIFICATION REQUEST message, the gNB-CU-UP shall update the corresponding information.

For each requested DRB, if the *PDCP Duplication* IE or *Additional PDCP duplication Information* IE is included in the *PDCP Configuration* IE contained in the BEARER CONTEXT MODIFICATION REQUEST message, then the gNB-CU-CP shall include two or more *UP Transport Layer Information* IEs in the BEARER CONTEXT MODIFICATION REQUEST message, and the gNB-CU-UP shall, if supported, also include two or more *UP Transport Layer Information* IEs in the BEARER CONTEXT MODIFICATION RESPONSE message to support packet duplication. If only one cell group is included in the *Cell Group Information* IE for the concerned DRB, then the gNB-CU-UP shall consider that the first *UP Transport Layer Information* IE of these *UP Transport Layer Information* IEs is for the primary path. If more than one cell group is included in the *Cell Group Information* IE, then the gNB-CU-UP shall consider that the number of duplication tunnels for each cell group is indicated by the *Numbe*r *of tunnels* IE, and that the first *UP Transport Layer Information* IE for each cell group is for the primary path or the split secondary path.

For a certain DRB which was allocated with two or more GTP-U tunnels, if such DRB is modified and given one GTP-U tunnel via the Bearer Context Modification (gNB-CU-CP initiated) procedure, i.e. only one UP Transport Layer Information per Cell Group ID is present in *DL UP Parameters* IE for the concerned DRB, then the gNB-CU-UP shall consider that PDCP duplication is deconfigured for this DRB. If such Bearer Context Modification (gNB-CU-CP initiated) procedure occurs, the *Duplication Activation* IE shall not be included for the concerned DRB.

If the *New UL TNL Information Required* IE is contained in the BEARER CONTEXT MODIFICATION REQUEST message, the gNB-CU-UP shall include the new UP Transport Layer Information in the BEARER CONTEXT MODIFICATION RESPONSE message.

For each PDU session for which the *Security Indication* IE is included in the *PDU Session Resource To Setup List* IE or the *Security Indication Modify* IE is included in the *PDU Session Resource To Modify List* IE of the BEARER CONTEXT MODIFICATION REQUEST message, and the *Integrity Protection Indication* IE or *Confidentiality Protection Indication* IE is set to "preferred", then the gNB-CU-UP should, if supported, perform user plane integrity protection or ciphering, respectively, for the concerned PDU session and shall notify whether it performed the user plane integrity protection or ciphering by including the *Integrity Protection Result* IE or *Confidentiality Protection Result* IE, respectively, in the *PDU Session Resource Setup List* IE or the *PDU Session Resource Modified List* IE of the BEARER CONTEXT MODIFICATION RESPONSE message.

For each PDU session for which the *Security Indication* IE is included in the *PDU Session Resource To Setup List* IE or the *Security Indication Modify* IE is included in the *PDU Session Resource To Modify List* IE of the BEARER CONTEXT MODIFICATION REQUEST message, and the *Integrity Protection Indication* IE or *Confidentiality Protection Indication* IE is set to "required", then the gNB-CU-UP shall perform user plane integrity protection or ciphering, respectively, for the concerned PDU Session. If the gNB-CU-UP cannot perform the user plane integrity protection or ciphering, it shall reject the setup of the PDU Session Resources with an appropriate cause value.

For each PDU session for which the Security Indication IE is included in the *PDU Session Resource To Setup List* IE or the *Security Indication Modify* IE is included in the *PDU Session Resource To Modify List* IE of the BEARER CONTEXT MODIFICATION REQUEST message:

- if the *Integrity Protection Indication* IE is set to "not needed", then the gNB-CU-UP shall not perform user plane integrity protection for the concerned PDU session;

-if the *Confidentiality Protection Indication* IE is set to "not needed", then the gNB-CU-UP shall not perform user plane ciphering for the concerned PDU session.

For each PDU Session Resource, if the *Network Instance* IE is included in the *PDU Session Resource To Setup List* IE or the *PDU Session Resource To Modify List* IE in the BEARER CONTEXT MODIFICATION REQUEST message and the *Common Network Instance* IE is not included, the gNB-CU-UP shall, if supported, use it when selecting transport network resource as specified in TS 23.501 [20].

For each PDU session, if the *Common Network Instance* IE is included in the *PDU Session Resource To Setup List* IE or the *PDU Session Resource To Modify List* IE in the BEARER CONTEXT MODIFICATION REQUEST message, the gNB-CU-UP shall, if supported, use it when selecting transport network resource as specified in TS 23.501 [20].

For each PDU session, if the *Redundant NG UL UP Transport Layer Information* IE is included in the *PDU Session Resource To Setup List* IE or the *PDU Session Resource To Modify List* IE in the BEARER CONTEXT MODIFICATION REQUEST message, the gNB-CU-UP shall, if supported, include the *Redundant NG DL UP Transport Layer Information* IE in the *PDU Session Resource Setup List* IE or the *PDU Session Resource Modified List* IE in the BEARER CONTEXT MODIFICATION RESPONSE message.

If the *Redundant Common Network Instance* IE is included in the *PDU Session Resource To Setup List* IE or the *PDU Session Resource To Modify List* IE in the BEARER CONTEXT MODIFICATION REQUEST message, the gNB-CU-UP shall, if supported, use it when selecting transport network resource for the redundant transmission as specified in TS 23.501 [20].

For each PDU session for which the *Redundant QoS Flow Indicator* IE is included in *QoS Flows Information To Be Setup* IE contained in the BEARER CONTEXT MODIFICATION REQUEST message, the gNB-CU-UP shall, if support, shall store and use it as specified in TS 23.501 [20].

For each PDU session, if the *Redundant QoS Flow Indicator* IE is set to false for all QoS flows, the gNB-CU-UP shall, if supported, stop the redundant transmission and release the redundant tunnel for the concerned PDU session as specified in TS 23.501 [20].

If the *QoS Flow Mapping Indication* IE is contained in the *QoS Flow QoS Parameters List* IE in the BEARER CONTEXT MODIFICATION REQUEST message, the gNB-CU-UP shall, if supported, replace any previously received value and take it into account that only the uplink or downlink QoS flow is mapped to the DRB.

If the *Data Discard Required* IE is contained in the BEARER CONTEXT MODIFICATION REQUEST message and the value is set to “Required”, the gNB-CU-UP shall consider that a RAN Paging Failure occurred for that UE. The gNB-CU-UP shall discard the user plane data for that UE and consider that the bearer context is still suspended.

If *UE Inactivity Timer* IE or *PDU session Inactivity Timer* IE or *DRB Inactivity Timer* IE is contained in BEARER CONTEXT MODIFICATION REQUEST message, the gNB-CU-UP shall take it into account when perform inactivity monitoring.

If the *S-NSSAI* IE is contained in the *PDU Session Resource To Modify List* IE in the BEARER CONTEXT MODIFICATION REQUEST message, the gNB-CU-UP shall store the corresponding information and replace any existing information.

If the *DRB QoS* IE is contained within the *DRB To Setup List* IE in the BEARER CONTEXT MODIFICATION REQUEST message, the gNB-CU-UP shall, if supported, take it into account for each DRB, as specified in TS 28.552 [22].

If the *DRB QoS* IE is contained within the *DRB To Modify List* IE in the BEARER CONTEXT MODIFICATION REQUEST message, the gNB-CU-UP shall, if supported, replace any previously received value and take it into account for each DRB, as specifed in TS 28.552 [22].

If the *gNB-DU-ID* IE is contained in the BEARER CONTEXT MODIFICATION REQUEST message, the gNB-CU-UP shall store and replace any previous information received.

If the *RAN UE ID* IE is contained in the BEARER CONTEXT MODIFICATION REQUEST message, the gNB-CU-UP shall store and replace any previous information received.

If the gNB-CU-UP receives a BEARER CONTEXT MODIFICATION REQUEST message including *Activity Notification Level* IE and its value does not match the current bearer context, the gNB-CU-UP shall ignore the *Activity Notification Level* IE and also the requested modification of inactivity timer.

If the *Handover With Full Configuration* IE is contained in the BEARER CONTEXT MODIFICATION REQUEST message and is set to “true”, the gNB-CU-UP shall, if supported, reset the PDCP Count for the relevant DRBs (i.e. set its HFN and PDCP-SN to value “0”).

For each successfully established DRB, the gNB-CU-UP shall provide, in the respective *UL UP Parameters* IE of the BEARER CONTEXT MODIFICATION RESPONSE, one UL UP Transport Layer Information Item per cell group entry contained in the respective *Cell Group Information* IE of the BEARER CONTEXT MODIFICATION REQUEST message.

If the *Old QoS Flow List - UL End Marker expected* IE is included in the *PDU Session Resource To Modify List* IE of the BEARER CONTEXT MODIFICATION REQUEST message for a DRB to be modified, the gNB-CU-UP shall consider that the source NG-RAN node has initiated QoS flow re-mapping and has not yet received SDAP end markers, as described in TS 38.300 [8]. The gNB-CU-UP shall consider that the *Old QoS Flow List - UL End Marker expected* IE only contains UL QoS flow information for QoS flows for which no SDAP end marker has been yet received on the source side.

For EN-DC, if the *Subscriber Profile ID for RAT/Frequency priority* IE is included in the BEARER CONTEXT MODIFICATION REQUEST, the gNB-CU-UP may use it to apply specific RRM policies as specified in TS 36.300 [25]. If the *Additional RRM Policy Index* IE is included in the BEARER CONTEXT MODIFICATION REQUEST, the gNB-CU-UP may use it to apply specific RRM policies as specified in TS 36.300 [25].

If there is at least one DRB removed by the gNB-CU-UP, the gNB-CU-UP shall, if supported, include the *Retainability Measurements Information* IE in the BEARER CONTEXT MODIFICATION RESPONSE message, providing information on the removed DRB(s) for retainability measurements in the gNB-CU-CP, as described in TS 32.425 [26] and TS 28.552 [22].

If the *TSC Traffic Characteristics* IE is included in the BEARER CONTEXT MODIFICATION REQUEST message, the gNB-CU-UP shall, if supported, take into account the corresponding information received in the *TSC Traffic Characteristics* IE.

For each QoS flow whose DRB has been successfully established or modified and the *QoS Monitoring Request* IE was included in the *QoS Flow Level QoS Parameters* IE contained in the BEARER CONTEXT MODIFICATION REQUEST message, the gNB-CU-UP shall store this information, and, if supported, perform delay measurement and QoS monitoring, as specified in TS 23.501 [20]. If the *QoS Monitoring Reporting Frequency* IE was included in the *QoS Flow Level QoS Parameters* IE contained in the BEARER CONTEXT MODIFICATION REQUEST message, the gNB-CU-UP shall store this information, and, if supported, use it for RAN part delay reporting.

For each requested DRB, if the *QoS Mapping Information* IE is contained in the *DL UP Parameters* IE in the BEARER CONTEXT MODIFICATION REQUEST message, the gNB-CU-UP shall use it to set DSCP and/or flow label fields in the downlink IP packets which are transmitted through the GTP tunnels indicated by the *UP Transport Layer Information* IE. The Diffserv code point (DSCP) marking is performed as specified in TS 38.474 [28].

If the *Early Forwarding COUNT Request* IE is contained in the *DRB To Modify List* IE in the BEARER CONTEXT MODIFICATION REQUEST message, the gNB-CU-UP shall act as specified in TS 38.401 [2] and include the requested *FIRST DL COUNT Value* IE or *DISCARD DL COUNT Value* IE in the BEARER CONTEXT MODIFICATION RESPONSE message.

If the *Early Forwarding COUNT Information* IE is contained in the *DRB To Modify List* IE in the BEARER CONTEXT MODIFICATION REQUEST message, the gNB-CU-UP shall take it into account and act as specified in TS 38.401 [2].

If the *Ignore Mapping Rule Indication* IE is contained within the *DRB To Setup List* IE for a DRB in the BEARER CONTEXT MODIFICATION REQUEST message, the gNB-CU-UP shall, if supported, ignore the QoS flow mapping information indicated by the *QoS Flows Information To Be Setup* IE for the concerned DRB.

If the *DAPS Request Information* IE is included for a DRB to be modified in the BEARER CONTEXT MODIFICATION REQUEST message, the gNB-CU-UP shall consider that the request concerns a DAPS handover for that DRB and, if admitted, act as specified in TS 38.300 [4].

If the *Early Data Forwarding Indicator* IE set to “stop” is contained in the *DRB To Modify List* IE in the BEARER CONTEXT MODIFICATION REQUEST message, the gNB-CU-UP shall, if supported and if already initiated, stop the early data forwarding for the concerned DRB. If the *DRB Data forwarding information* IE containing the *DL Data Forwarding* IE is included together in the *DRB To Modify List* IE, the gNB-CU-UP shall consider that the stop is only for the early data forwarding initiated toward that forwarding TNL.

If the *Data Forwarding* *Source IP Address* IE is included in the *DRB To Setup Modification List E-UTRAN* IE or in the *QoS Flow Level QoS Parameters* IE within the *PDU Session Resource To Setup Modification List* IE and the *PDU Session Resource To Modify List* IE contained in the BEARER CONTEXT MODIFICATION REQUEST message, the gNB-CU-UP shall, if supported, store this information in the UE context and use it as part of its ACL functionality configuration actions, if such ACL functionality is deployed.

If the *Data Forwarding* *Source IP Address* IE is included in the *DRB Setup Modification List E-UTRAN* IE or in the *Flow Setup List* IE within the *PDU Session Resource Setup Modification List* IE and the *PDU Session Resource Modified List* IE of the BEARER CONTEXT MODIFICATION RESPONSE message, the gNB-CU-CP shall, if supported, store this information in the UE context and use it as part of its ACL functionality configuration actions, if such ACL functionality is deployed.

**Interaction with the Bearer Context Modification (gNB-CU-CP initiated)**

If the BEARER CONTEXT MODIFICATION REQUEST message includes for a DRB in the *DRB To Modify List* IE the *PDCP SN Status Request IE* set to “requested” and if the gNB-CU-UP has not yet received a SDAP end marker packet for a QoS flow which has been previously re-configured to another DRB by means of a gNB-CU-CP initiated Bearer Context Modification procedure, the gNB-CU-UP shall includes the QoS Flow Identifier of that QoS flow in the *Old QoS Flow List - UL End Marker expected* IE in the *PDU Session Resource Modified List* IE in the BEARER CONTEXT MODIFICATION RESPONSE message.

#### 8.3.2.3 Unsuccessful Operation



Figure 8.3.2.3-1: Bearer Context Modification procedure: Unsuccessful Operation.

If the gNB-CU-UP cannot successfully perform any of the requested bearer context modifications, it shall respond with a BEARER CONTEXT MODIFICATION FAILURE message and appropriate cause value.

If the gNB-CU-UP receives a BEARER CONTEXT MODIFICATION REQUEST message containing the *Security Indication Modify* IE in the *PDU Session Resource To Modify List* IE for a PDU session that may result in the change of security status that has been applied but the DRBs that have been established for that PDU session are not requested to be released via the *DRB To Remove List* IEs as specified in TS 38.331 [10], then the gNB-CU-UP shall respond with a BEARER CONTEXT MODIFICATION FAILURE message and appropriate cause value.

#### 8.3.2.4 Abnormal Conditions

If the gNB-CU-UP receives a BEARER CONTEXT MODIFICATION REQUEST message containing a *E-UTRAN QoS* IE in the *DRB To Setup List* or the *DRB To Modify List* IE for a GBR QoS DRB but where the *GBR QoS Information* IE is not present, the gNB-CU-UP shall report the addition or the modification of the corresponding DRB as failed in the *DRB Failed List* IE or the *DRB Failed To Modify List* IE of the BEARER CONTEXT MODIFICATION RESPONSE message with an appropriate cause value.

If the gNB-CU-UP receives a BEARER CONTEXT MODIFICATION REQUEST message containing a *QoS Flow Level QoS Parameters* IE in the *PDU Session Resource To Setup List* IE or the *PDU Session Resource To Modify List* IE for a GBR QoS Flow but where the *GBR QoS Flow Information* IE is not present, the gNB-CU-UP shall report the addition or the modification of the corresponding QoS Flow as failed in the corresponding *Flow Failed List* IE of the BEARER CONTEXT MODIFICATION RESPONSE message with an appropriate cause value.

<<<<<<<<<<<<<<<<<<<< Next Change >>>>>>>>>>>>>>>>>>>>

#### 9.2.2.4 BEARER CONTEXT MODIFICATION REQUEST

This message is sent by the gNB-CU-CP to request the gNB-CU-UP to modify a bearer context.

Direction: gNB-CU-CP → gNB-CU-UP

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| Message Type | M |  | 9.3.1.1 |  | YES | reject |
| gNB-CU-CP UE E1AP ID | M |  | 9.3.1.4 |  | YES | reject |
| gNB-CU-UP UE E1AP ID | M |  | 9.3.1.5 |  | YES | reject |
| Security Information | O |  | 9.3.1.10 |  | YES | reject |
| UE DL Aggregate Maximum Bit Rate | O |  | Bit Rate 9.3.1.20 |  | YES | reject |
| UE DL Maximum Integrity Protected Data Rate | O |  | Bit Rate 9.3.1.20 | The Bit Rate is a portion of the UE’s Maximum Integrity Protected Data Rate, and is enforced by the gNB-CU-UP node. | YES | reject |
| Bearer Context Status Change | O |  | ENUMERATED (Suspend, Resume, …) | Indicates the status of the Bearer Context | YES | reject |
| New UL TNL Information Required | O |  | ENUMERATED (required, …) | Indicates that new UL TNL information has been requested to be provided. | YES | reject |
| UE Inactivity Timer | O |  | Inactivity Timer 9.3.1.54 | Included if the Activity Notification Level is set to UE. | - | - |
| Data Discard Required | O |  | ENUMERATED (required, …) | Indicate to discard the DL user data in case of RAN paging failure. | YES | ignore |
| CHOICE *System* | O |  |  |  | YES | reject |
| *>E-UTRAN* |  |  |  |  |  |  |
| >>DRB To Setup List | O |  | DRB To Setup Modification List E-UTRAN 9.3.3.7 |  | YES | reject |
| >>DRB To Modify List | O |  | DRB To Modify List E-UTRAN9.3.3.8 |  | YES | reject |
| >>DRB To Remove List | O |  | DRB To Remove List E-UTRAN 9.3.3.9 |  | YES | reject |
| >>Subscriber Profile ID for RAT/Frequency priority | O |  | 9.3.1.69 |  | YES | ignore |
| >>Additional RRM Policy Index | O |  | 9.3.1.70 |  | YES | ignore |
| *>NG-RAN* |  |  |  |  |  |  |
| >>PDU Session Resource To Setup List | O |  | PDU Session Resource To Setup Modification List9.3.3.10 |  | YES | reject |
| >>PDU Session Resource To Modify List | O |  | 9.3.3.11 |  | YES | reject |
| >>PDU Session Resource To Remove List | O |  | 9.3.3.12 |  | YES | reject |
| RAN UE ID | O |  | OCTET STRING (SIZE(8)) |  | YES | ignore |
| gNB-DU ID | O |  | 9.3.1.65 |  | YES | ignore |
| Activity Notification Level | O |  | 9.3.1.67 |  | YES | ignore |
| Handover With Full Configuration | O |  | ENUMERATED (True, …) |  | YES | reject |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofDRBs | Maximum no. of DRBs for a UE. Value is 32. |
| maxnoofPDUSessionResource  | Maximum no. of PDU Sessions for a UE. Value is 256. |

<<<<<<<<<<<<<<<<<<<< Next Change >>>>>>>>>>>>>>>>>>>>

### 9.4.4 PDU Definitions

-- ASN1START

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- PDU definitions for E1AP

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

E1AP-PDU-Contents {

itu-t (0) identified-organization (4) etsi (0) mobileDomain (0)

ngran-access (22) modules (3) e1ap (5) version1 (1) e1ap-PDU-Contents (1) }

DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- IE parameter types from other modules

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

IMPORTS

 Cause,

 CriticalityDiagnostics,

 GNB-CU-CP-UE-E1AP-ID,

 GNB-CU-UP-UE-E1AP-ID,

 UE-associatedLogicalE1-ConnectionItem,

 GNB-CU-UP-ID,

 GNB-CU-UP-Name,

 Extended-GNB-CU-UP-Name,

 GNB-CU-CP-Name,

 Extended-GNB-CU-CP-Name,

 CNSupport,

 PLMN-Identity,

 Slice-Support-List,

 NR-CGI-Support-List,

 QoS-Parameters-Support-List,

 SecurityInformation,

 BitRate,

 BearerContextStatusChange,

 DRB-To-Setup-List-EUTRAN,

 DRB-Setup-List-EUTRAN,

 DRB-Failed-List-EUTRAN,

 DRB-To-Modify-List-EUTRAN,

 DRB-Measurement-Results-Information-List,

 DRB-Modified-List-EUTRAN,

 DRB-Failed-To-Modify-List-EUTRAN,

 DRB-To-Remove-List-EUTRAN,

 DRB-Required-To-Remove-List-EUTRAN,

 DRB-Required-To-Modify-List-EUTRAN,

 DRB-Confirm-Modified-List-EUTRAN,

 DRB-To-Setup-Mod-List-EUTRAN,

 DRB-Setup-Mod-List-EUTRAN,

 DRB-Failed-Mod-List-EUTRAN,

 ExtendedSliceSupportList,

 PDU-Session-Resource-To-Setup-List,

 PDU-Session-Resource-Setup-List,

 PDU-Session-Resource-Failed-List,

 PDU-Session-Resource-To-Modify-List,

 PDU-Session-Resource-Modified-List,

 PDU-Session-Resource-Failed-To-Modify-List,

 PDU-Session-Resource-To-Remove-List,

 PDU-Session-Resource-Required-To-Modify-List,

 PDU-Session-Resource-Confirm-Modified-List,

 PDU-Session-Resource-To-Setup-Mod-List,

 PDU-Session-Resource-Setup-Mod-List,

 PDU-Session-Resource-Failed-Mod-List,

 PDU-Session-To-Notify-List,

 DRB-Status-Item,

 DRB-Activity-Item,

 Data-Usage-Report-List,

 TimeToWait,

 ActivityNotificationLevel,

 ActivityInformation,

 New-UL-TNL-Information-Required,

 GNB-CU-CP-TNLA-Setup-Item,

 GNB-CU-CP-TNLA-Failed-To-Setup-Item,

 GNB-CU-CP-TNLA-To-Add-Item,

 GNB-CU-CP-TNLA-To-Remove-Item,

 GNB-CU-CP-TNLA-To-Update-Item,

 GNB-CU-UP-TNLA-To-Remove-Item,

 TransactionID,

 Inactivity-Timer,

 DRBs-Subject-To-Counter-Check-List-EUTRAN,

 DRBs-Subject-To-Counter-Check-List-NG-RAN,

 PPI,

 GNB-CU-UP-Capacity,

 GNB-CU-UP-OverloadInformation,

 DataDiscardRequired,

 PDU-Session-Resource-Data-Usage-List,

 RANUEID,

 GNB-DU-ID,

 TraceID,

 TraceActivation,

 SubscriberProfileIDforRFP,

 AdditionalRRMPriorityIndex,

 RetainabilityMeasurementsInfo,

 Transport-Layer-Address-Info,

 HW-CapacityIndicator,

 RegistrationRequest,

 ReportCharacteristics,

 ReportingPeriodicity,

 TNL-AvailableCapacityIndicator,

 DLUPTNLAddressToUpdateItem,

 ULUPTNLAddressToUpdateItem,

 NPNContextInfo,

 NPNSupportInfo,

 MDTPLMNList,

 PrivacyIndicator,

 URIaddress,

 DRBs-Subject-To-Early-Forwarding-List,

 CHOInitiation,

 ExtendedSliceSupportList,

 TransportLayerAddress,

 AdditionalHandoverInfo,

 Extended-NR-CGI-Support-List,

 DirectForwardingPathAvailability,

 IAB-Donor-CU-UPPSKInfo-Item,

 Handover-With-Full-Configuration

FROM E1AP-IEs

 PrivateIE-Container{},

 ProtocolExtensionContainer{},

 ProtocolIE-Container{},

 ProtocolIE-ContainerList{},

 ProtocolIE-SingleContainer{},

 E1AP-PRIVATE-IES,

 E1AP-PROTOCOL-EXTENSION,

 E1AP-PROTOCOL-IES

FROM E1AP-Containers

 id-Cause,

 id-CriticalityDiagnostics,

 id-gNB-CU-CP-UE-E1AP-ID,

 id-gNB-CU-UP-UE-E1AP-ID,

 id-ResetType,

 id-UE-associatedLogicalE1-ConnectionItem,

 id-UE-associatedLogicalE1-ConnectionListResAck,

 id-gNB-CU-UP-ID,

 id-gNB-CU-UP-Name,

 id-Extended-GNB-CU-UP-Name,

 id-gNB-CU-CP-Name,

 id-Extended-GNB-CU-CP-Name,

 id-CNSupport,

 id-SupportedPLMNs,

 id-NPNSupportInfo,

 id-NPNContextInfo,

 id-SecurityInformation,

 id-UEDLAggregateMaximumBitRate,

 id-BearerContextStatusChange,

 id-System-BearerContextSetupRequest,

 id-System-BearerContextSetupResponse,

 id-System-BearerContextModificationRequest,

 id-System-BearerContextModificationResponse,

 id-System-BearerContextModificationConfirm,

 id-System-BearerContextModificationRequired,

 id-DRB-Status-List,

 id-Data-Usage-Report-List,

 id-TimeToWait,

 id-ActivityNotificationLevel,

 id-ActivityInformation,

 id-New-UL-TNL-Information-Required,

 id-GNB-CU-CP-TNLA-Setup-List,

 id-GNB-CU-CP-TNLA-Failed-To-Setup-List,

 id-GNB-CU-CP-TNLA-To-Add-List,

 id-GNB-CU-CP-TNLA-To-Remove-List,

 id-GNB-CU-CP-TNLA-To-Update-List,

 id-GNB-CU-UP-TNLA-To-Remove-List,

 id-DRB-To-Setup-List-EUTRAN,

 id-DRB-To-Modify-List-EUTRAN,

 id-DRB-To-Remove-List-EUTRAN,

 id-DRB-Required-To-Modify-List-EUTRAN,

 id-DRB-Required-To-Remove-List-EUTRAN,

 id-DRB-Setup-List-EUTRAN,

 id-DRB-Failed-List-EUTRAN,

 id-DRB-Measurement-Results-Information-List,

 id-DRB-Modified-List-EUTRAN,

 id-DRB-Failed-To-Modify-List-EUTRAN,

 id-DRB-Confirm-Modified-List-EUTRAN,

 id-DRB-To-Setup-Mod-List-EUTRAN,

 id-DRB-Setup-Mod-List-EUTRAN,

 id-DRB-Failed-Mod-List-EUTRAN,

 id-PDU-Session-Resource-To-Setup-List,

 id-PDU-Session-Resource-To-Modify-List,

 id-PDU-Session-Resource-To-Remove-List,

 id-PDU-Session-Resource-Required-To-Modify-List,

 id-PDU-Session-Resource-Setup-List,

 id-PDU-Session-Resource-Failed-List,

 id-PDU-Session-Resource-Modified-List,

 id-PDU-Session-Resource-Failed-To-Modify-List,

 id-PDU-Session-Resource-Confirm-Modified-List,

 id-PDU-Session-Resource-Setup-Mod-List,

 id-PDU-Session-Resource-Failed-Mod-List,

 id-PDU-Session-Resource-To-Setup-Mod-List,

 id-PDU-Session-To-Notify-List,

 id-TransactionID,

 id-Serving-PLMN,

 id-UE-Inactivity-Timer,

 id-System-GNB-CU-UP-CounterCheckRequest,

 id-DRBs-Subject-To-Counter-Check-List-EUTRAN,

 id-DRBs-Subject-To-Counter-Check-List-NG-RAN,

 id-PPI,

 id-gNB-CU-UP-Capacity,

 id-GNB-CU-UP-OverloadInformation,

 id-UEDLMaximumIntegrityProtectedDataRate,

 id-DataDiscardRequired,

 id-PDU-Session-Resource-Data-Usage-List,

 id-RANUEID,

 id-GNB-DU-ID,

 id-TraceID,

 id-TraceActivation,

 id-SubscriberProfileIDforRFP,

 id-AdditionalRRMPriorityIndex,

 id-RetainabilityMeasurementsInfo,

 id-Transport-Layer-Address-Info,

 id-gNB-CU-CP-Measurement-ID,

 id-gNB-CU-UP-Measurement-ID,

 id-RegistrationRequest,

 id-ReportCharacteristics,

 id-ReportingPeriodicity,

 id-TNL-AvailableCapacityIndicator,

 id-HW-CapacityIndicator,

 id-DLUPTNLAddressToUpdateList,

 id-ULUPTNLAddressToUpdateList,

 id-ManagementBasedMDTPLMNList,

 id-TraceCollectionEntityIPAddress,

 id-PrivacyIndicator,

 id-URIaddress,

 id-DRBs-Subject-To-Early-Forwarding-List,

 id-CHOInitiation,

 id-ExtendedSliceSupportList,

 id-AdditionalHandoverInfo,

 id-Extended-NR-CGI-Support-List,

 id-DirectForwardingPathAvailability,

 id-IAB-Donor-CU-UPPSKInfo,

 id-Handover-With-Full-Configuration,

 maxnoofErrors,

 maxnoofSPLMNs,

 maxnoofDRBs,

 maxnoofTNLAssociations,

 maxnoofIndividualE1ConnectionsToReset,

 maxnoofTNLAddresses,

 maxnoofPSKs

FROM E1AP-Constants;

<<<<<<<<<<<<<<<<<<<< Next Change >>>>>>>>>>>>>>>>>>>>

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- BEARER CONTEXT MODIFICATION

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Bearer Context Modification Request

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

BearerContextModificationRequest ::= SEQUENCE {

 protocolIEs ProtocolIE-Container { { BearerContextModificationRequestIEs} },

 ...

}

BearerContextModificationRequestIEs E1AP-PROTOCOL-IES ::= {

 { ID id-gNB-CU-CP-UE-E1AP-ID CRITICALITY reject TYPE GNB-CU-CP-UE-E1AP-ID PRESENCE mandatory }|

 { ID id-gNB-CU-UP-UE-E1AP-ID CRITICALITY reject TYPE GNB-CU-UP-UE-E1AP-ID PRESENCE mandatory }|

 { ID id-SecurityInformation CRITICALITY reject TYPE SecurityInformation PRESENCE optional }|

 { ID id-UEDLAggregateMaximumBitRate CRITICALITY reject TYPE BitRate PRESENCE optional }|

 { ID id-UEDLMaximumIntegrityProtectedDataRate CRITICALITY reject TYPE BitRate PRESENCE optional }|

 { ID id-BearerContextStatusChange CRITICALITY reject TYPE BearerContextStatusChange PRESENCE optional }|

 { ID id-New-UL-TNL-Information-Required CRITICALITY reject TYPE New-UL-TNL-Information-Required PRESENCE optional }|

 { ID id-UE-Inactivity-Timer CRITICALITY reject TYPE Inactivity-Timer PRESENCE optional }|

 { ID id-DataDiscardRequired CRITICALITY ignore TYPE DataDiscardRequired PRESENCE optional }|

 { ID id-System-BearerContextModificationRequest CRITICALITY reject TYPE System-BearerContextModificationRequest PRESENCE optional }|

 { ID id-RANUEID CRITICALITY ignore TYPE RANUEID PRESENCE optional }|

 { ID id-GNB-DU-ID CRITICALITY ignore TYPE GNB-DU-ID PRESENCE optional }|

 { ID id-ActivityNotificationLevel CRITICALITY ignore TYPE ActivityNotificationLevel PRESENCE optional } |

 { ID id-Handover-With-Full-Configuration CRITICALITY reject TYPE Handover-With-Full-Configuration PRESENCE optional },

 ...

}

System-BearerContextModificationRequest ::= CHOICE {

 e-UTRAN-BearerContextModificationRequest ProtocolIE-Container {{EUTRAN-BearerContextModificationRequest}},

 nG-RAN-BearerContextModificationRequest ProtocolIE-Container {{NG-RAN-BearerContextModificationRequest}},

 choice-extension ProtocolIE-SingleContainer {{System-BearerContextModificationRequest-ExtIEs}}

}

System-BearerContextModificationRequest-ExtIEs E1AP-PROTOCOL-IES ::= {

 ...

}

EUTRAN-BearerContextModificationRequest E1AP-PROTOCOL-IES ::= {

 { ID id-DRB-To-Setup-Mod-List-EUTRAN CRITICALITY reject TYPE DRB-To-Setup-Mod-List-EUTRAN PRESENCE optional }|

 { ID id-DRB-To-Modify-List-EUTRAN CRITICALITY reject TYPE DRB-To-Modify-List-EUTRAN PRESENCE optional }|

 { ID id-DRB-To-Remove-List-EUTRAN CRITICALITY reject TYPE DRB-To-Remove-List-EUTRAN PRESENCE optional }|

 { ID id-SubscriberProfileIDforRFP CRITICALITY ignore TYPE SubscriberProfileIDforRFP PRESENCE optional }|

 { ID id-AdditionalRRMPriorityIndex CRITICALITY ignore TYPE AdditionalRRMPriorityIndex PRESENCE optional },

 ...

}

NG-RAN-BearerContextModificationRequest E1AP-PROTOCOL-IES ::= {

 { ID id-PDU-Session-Resource-To-Setup-Mod-List CRITICALITY reject TYPE PDU-Session-Resource-To-Setup-Mod-List PRESENCE optional }|

 { ID id-PDU-Session-Resource-To-Modify-List CRITICALITY reject TYPE PDU-Session-Resource-To-Modify-List PRESENCE optional }|

 { ID id-PDU-Session-Resource-To-Remove-List CRITICALITY reject TYPE PDU-Session-Resource-To-Remove-List PRESENCE optional },

 ...

}

<<<<<<<<<<<<<<<<<<<< Next Change >>>>>>>>>>>>>>>>>>>>

### 9.4.5 Information Element Definitions

-- ASN1START

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Information Element Definitions

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

E1AP-IEs {

itu-t (0) identified-organization (4) etsi (0) mobileDomain (0)

ngran-access (22) modules (3) e1ap (5) version1 (1) e1ap-IEs (2) }

DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

IMPORTS

 id-CommonNetworkInstance,

 id-SNSSAI,

 id-OldQoSFlowMap-ULendmarkerexpected,

 id-DRB-QoS,

 id-endpoint-IP-Address-and-Port,

 id-NetworkInstance,

 id-QoSFlowMappingIndication,

 id-TNLAssociationTransportLayerAddressgNBCUUP,

 id-Cause,

 id-QoSMonitoringRequest,

 id-QosMonitoringReportingFrequency,

 id-QoSMonitoringDisabled,

 id-PDCP-StatusReportIndication,

 id-RedundantCommonNetworkInstance,

 id-redundant-nG-UL-UP-TNL-Information,

 id-redundant-nG-DL-UP-TNL-Information,

 id-RedundantQosFlowIndicator,

 id-TSCTrafficCharacteristics,

 id-ExtendedPacketDelayBudget,

 id-CNPacketDelayBudgetDownlink,

 id-CNPacketDelayBudgetUplink,

 id-AdditionalPDCPduplicationInformation,

 id-RedundantPDUSessionInformation,

 id-RedundantPDUSessionInformation-used,

 id-QoS-Mapping-Information,

 id-MDTConfiguration,

 id-TraceCollectionEntityURI,

 id-EHC-Parameters,

 id-DAPSRequestInfo,

 id-EarlyForwardingCOUNTReq,

 id-EarlyForwardingCOUNTInfo,

 id-AlternativeQoSParaSetList,

 id-MCG-OfferedGBRQoSFlowInfo,

 id-Number-of-tunnels,

 id-DataForwardingtoE-UTRANInformationList,

 id-DataForwardingtoNG-RANQoSFlowInformationList,

 id-MaxCIDEHCDL,

 id-ignoreMappingRuleIndication,

 id-EarlyDataForwardingIndicator,

 id-QoSFlowsDRBRemapping,

 id-SecurityIndicationModify,

 id-DataForwardingSourceIPAddress,

 id-DiscardTimerExtended,

 id-Haandover-With-FullConfiguration,

 maxnoofQoSParaSets,

 maxnoofErrors,

 maxnoofSliceItems,

 maxnoofEUTRANQOSParameters,

 maxnoofNGRANQOSParameters,

 maxnoofDRBs,

 maxnoofPDUSessionResource,

 maxnoofQoSFlows,

 maxnoofUPParameters,

 maxnoofCellGroups,

 maxnooftimeperiods,

 maxnoofNRCGI,

 maxnoofTLAs,

 maxnoofGTPTLAs,

 maxnoofSPLMNs,

 maxnoofMDTPLMNs,

 maxnoofExtSliceItems,

 maxnoofDataForwardingTunneltoE-UTRAN,

 maxnoofExtNRCGI

FROM E1AP-Constants

 Criticality,

 ProcedureCode,

 ProtocolIE-ID,

 TriggeringMessage

FROM E1AP-CommonDataTypes

 ProtocolExtensionContainer{},

 ProtocolIE-SingleContainer{},

 E1AP-PROTOCOL-EXTENSION,

 E1AP-PROTOCOL-IES

FROM E1AP-Containers;

<<<<<<<<<<<<<<<<<<<< Next Change >>>>>>>>>>>>>>>>>>>>

-- H

Handover-with-Full-Configuration ::= ENUMERATED {

 true,

 ...

}

HFN ::= INTEGER (0..4294967295)

HW-CapacityIndicator ::= SEQUENCE {

 offeredThroughput INTEGER (1..16777216, ...),

 availableThroughput INTEGER (0..100, ...),

 iE-Extensions ProtocolExtensionContainer { { HW-CapacityIndicator-ExtIEs } },

 ...

}

HW-CapacityIndicator-ExtIEs E1AP-PROTOCOL-EXTENSION ::= {

 ...

}

-- I

<<<<<<<<<<<<<<<<<<<< Next Change >>>>>>>>>>>>>>>>>>>>

### 9.4.7 Constant Definitions

-- ASN1START

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Constant definitions

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

E1AP-Constants {

itu-t (0) identified-organization (4) etsi (0) mobileDomain (0)

ngran-access (22) modules (3) e1ap (5) version1 (1) e1ap-Constants (4) }

DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

IMPORTS

 ProcedureCode,

 ProtocolIE-ID

FROM E1AP-CommonDataTypes;

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Elementary Procedures

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

id-reset ProcedureCode ::= 0

id-errorIndication ProcedureCode ::= 1

id-privateMessage ProcedureCode ::= 2

id-gNB-CU-UP-E1Setup ProcedureCode ::= 3

id-gNB-CU-CP-E1Setup ProcedureCode ::= 4

id-gNB-CU-UP-ConfigurationUpdate ProcedureCode ::= 5

id-gNB-CU-CP-ConfigurationUpdate ProcedureCode ::= 6

id-e1Release ProcedureCode ::= 7

id-bearerContextSetup ProcedureCode ::= 8

id-bearerContextModification ProcedureCode ::= 9

id-bearerContextModificationRequired ProcedureCode ::= 10

id-bearerContextRelease ProcedureCode ::= 11

id-bearerContextReleaseRequest ProcedureCode ::= 12

id-bearerContextInactivityNotification ProcedureCode ::= 13

id-dLDataNotification ProcedureCode ::= 14

id-dataUsageReport ProcedureCode ::= 15

id-gNB-CU-UP-CounterCheck ProcedureCode ::= 16

id-gNB-CU-UP-StatusIndication ProcedureCode ::= 17

id-uLDataNotification ProcedureCode ::= 18

id-mRDC-DataUsageReport ProcedureCode ::= 19

id-TraceStart ProcedureCode ::= 20

id-DeactivateTrace ProcedureCode ::= 21

id-resourceStatusReportingInitiation ProcedureCode ::= 22

id-resourceStatusReporting ProcedureCode ::= 23

id-iAB-UPTNLAddressUpdate ProcedureCode ::= 24

id-CellTrafficTrace ProcedureCode ::= 25

id-earlyForwardingSNTransfer ProcedureCode ::= 26

id-gNB-CU-CPMeasurementResultsInformation ProcedureCode ::= 27

id-iABPSKNotification ProcedureCode ::= 28

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Lists

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

maxnoofErrors INTEGER ::= 256

maxnoofSPLMNs INTEGER ::= 12

maxnoofSliceItems INTEGER ::= 1024

maxnoofIndividualE1ConnectionsToReset INTEGER ::= 65536

maxnoofEUTRANQOSParameters INTEGER ::= 256

maxnoofNGRANQOSParameters INTEGER ::= 256

maxnoofDRBs INTEGER ::= 32

maxnoofNRCGI INTEGER ::= 512

maxnoofPDUSessionResource INTEGER ::= 256

maxnoofQoSFlows INTEGER ::= 64

maxnoofUPParameters INTEGER ::= 8

maxnoofCellGroups INTEGER ::= 4

maxnooftimeperiods INTEGER ::= 2

maxnoofTNLAssociations INTEGER ::= 32

maxnoofTLAs INTEGER ::= 16

maxnoofGTPTLAs INTEGER ::= 16

maxnoofTNLAddresses INTEGER ::= 8

maxnoofMDTPLMNs INTEGER ::= 16

maxnoofQoSParaSets INTEGER ::= 8

maxnoofExtSliceItems INTEGER ::= 65535

maxnoofDataForwardingTunneltoE-UTRAN INTEGER ::= 256

maxnoofExtNRCGI INTEGER ::= 16384

maxnoofPSKs INTEGER ::= 256

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- IEs

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

id-Cause ProtocolIE-ID ::= 0

id-CriticalityDiagnostics ProtocolIE-ID ::= 1

id-gNB-CU-CP-UE-E1AP-ID ProtocolIE-ID ::= 2

id-gNB-CU-UP-UE-E1AP-ID ProtocolIE-ID ::= 3

id-ResetType ProtocolIE-ID ::= 4

id-UE-associatedLogicalE1-ConnectionItem ProtocolIE-ID ::= 5

id-UE-associatedLogicalE1-ConnectionListResAck ProtocolIE-ID ::= 6

id-gNB-CU-UP-ID ProtocolIE-ID ::= 7

id-gNB-CU-UP-Name ProtocolIE-ID ::= 8

id-gNB-CU-CP-Name ProtocolIE-ID ::= 9

id-CNSupport ProtocolIE-ID ::= 10

id-SupportedPLMNs ProtocolIE-ID ::= 11

id-TimeToWait ProtocolIE-ID ::= 12

id-SecurityInformation ProtocolIE-ID ::= 13

id-UEDLAggregateMaximumBitRate ProtocolIE-ID ::= 14

id-System-BearerContextSetupRequest ProtocolIE-ID ::= 15

id-System-BearerContextSetupResponse ProtocolIE-ID ::= 16

id-BearerContextStatusChange ProtocolIE-ID ::= 17

id-System-BearerContextModificationRequest ProtocolIE-ID ::= 18

id-System-BearerContextModificationResponse ProtocolIE-ID ::= 19

id-System-BearerContextModificationConfirm ProtocolIE-ID ::= 20

id-System-BearerContextModificationRequired ProtocolIE-ID ::= 21

id-DRB-Status-List ProtocolIE-ID ::= 22

id-ActivityNotificationLevel ProtocolIE-ID ::= 23

id-ActivityInformation ProtocolIE-ID ::= 24

id-Data-Usage-Report-List ProtocolIE-ID ::= 25

id-New-UL-TNL-Information-Required ProtocolIE-ID ::= 26

id-GNB-CU-CP-TNLA-To-Add-List ProtocolIE-ID ::= 27

id-GNB-CU-CP-TNLA-To-Remove-List ProtocolIE-ID ::= 28

id-GNB-CU-CP-TNLA-To-Update-List ProtocolIE-ID ::= 29

id-GNB-CU-CP-TNLA-Setup-List ProtocolIE-ID ::= 30

id-GNB-CU-CP-TNLA-Failed-To-Setup-List ProtocolIE-ID ::= 31

id-DRB-To-Setup-List-EUTRAN ProtocolIE-ID ::= 32

id-DRB-To-Modify-List-EUTRAN ProtocolIE-ID ::= 33

id-DRB-To-Remove-List-EUTRAN ProtocolIE-ID ::= 34

id-DRB-Required-To-Modify-List-EUTRAN ProtocolIE-ID ::= 35

id-DRB-Required-To-Remove-List-EUTRAN ProtocolIE-ID ::= 36

id-DRB-Setup-List-EUTRAN ProtocolIE-ID ::= 37

id-DRB-Failed-List-EUTRAN ProtocolIE-ID ::= 38

id-DRB-Modified-List-EUTRAN ProtocolIE-ID ::= 39

id-DRB-Failed-To-Modify-List-EUTRAN ProtocolIE-ID ::= 40

id-DRB-Confirm-Modified-List-EUTRAN ProtocolIE-ID ::= 41

id-PDU-Session-Resource-To-Setup-List ProtocolIE-ID ::= 42

id-PDU-Session-Resource-To-Modify-List ProtocolIE-ID ::= 43

id-PDU-Session-Resource-To-Remove-List ProtocolIE-ID ::= 44

id-PDU-Session-Resource-Required-To-Modify-List ProtocolIE-ID ::= 45

id-PDU-Session-Resource-Setup-List ProtocolIE-ID ::= 46

id-PDU-Session-Resource-Failed-List ProtocolIE-ID ::= 47

id-PDU-Session-Resource-Modified-List ProtocolIE-ID ::= 48

id-PDU-Session-Resource-Failed-To-Modify-List ProtocolIE-ID ::= 49

id-PDU-Session-Resource-Confirm-Modified-List ProtocolIE-ID ::= 50

id-DRB-To-Setup-Mod-List-EUTRAN ProtocolIE-ID ::= 51

id-DRB-Setup-Mod-List-EUTRAN ProtocolIE-ID ::= 52

id-DRB-Failed-Mod-List-EUTRAN ProtocolIE-ID ::= 53

id-PDU-Session-Resource-Setup-Mod-List ProtocolIE-ID ::= 54

id-PDU-Session-Resource-Failed-Mod-List ProtocolIE-ID ::= 55

id-PDU-Session-Resource-To-Setup-Mod-List ProtocolIE-ID ::= 56

id-TransactionID ProtocolIE-ID ::= 57

id-Serving-PLMN ProtocolIE-ID ::= 58

id-UE-Inactivity-Timer ProtocolIE-ID ::= 59

id-System-GNB-CU-UP-CounterCheckRequest ProtocolIE-ID ::= 60

id-DRBs-Subject-To-Counter-Check-List-EUTRAN ProtocolIE-ID ::= 61

id-DRBs-Subject-To-Counter-Check-List-NG-RAN ProtocolIE-ID ::= 62

id-PPI ProtocolIE-ID ::= 63

id-gNB-CU-UP-Capacity ProtocolIE-ID ::= 64

id-GNB-CU-UP-OverloadInformation ProtocolIE-ID ::= 65

id-UEDLMaximumIntegrityProtectedDataRate ProtocolIE-ID ::= 66

id-PDU-Session-To-Notify-List ProtocolIE-ID ::= 67

id-PDU-Session-Resource-Data-Usage-List ProtocolIE-ID ::= 68

id-SNSSAI ProtocolIE-ID ::= 69

id-DataDiscardRequired ProtocolIE-ID ::= 70

id-OldQoSFlowMap-ULendmarkerexpected ProtocolIE-ID ::= 71

id-DRB-QoS ProtocolIE-ID ::= 72

id-GNB-CU-UP-TNLA-To-Remove-List ProtocolIE-ID ::= 73

id-endpoint-IP-Address-and-Port ProtocolIE-ID ::= 74

id-TNLAssociationTransportLayerAddressgNBCUUP ProtocolIE-ID ::= 75

id-RANUEID ProtocolIE-ID ::= 76

id-GNB-DU-ID ProtocolIE-ID ::= 77

id-CommonNetworkInstance ProtocolIE-ID ::= 78

id-NetworkInstance ProtocolIE-ID ::= 79

id-QoSFlowMappingIndication ProtocolIE-ID ::= 80

id-TraceActivation ProtocolIE-ID ::= 81

id-TraceID ProtocolIE-ID ::= 82

id-SubscriberProfileIDforRFP ProtocolIE-ID ::= 83

id-AdditionalRRMPriorityIndex ProtocolIE-ID ::= 84

id-RetainabilityMeasurementsInfo ProtocolIE-ID ::= 85

id-Transport-Layer-Address-Info ProtocolIE-ID ::= 86

id-QoSMonitoringRequest ProtocolIE-ID ::= 87

id-PDCP-StatusReportIndication ProtocolIE-ID ::= 88

id-gNB-CU-CP-Measurement-ID ProtocolIE-ID ::= 89

id-gNB-CU-UP-Measurement-ID ProtocolIE-ID ::= 90

id-RegistrationRequest ProtocolIE-ID ::= 91

id-ReportCharacteristics ProtocolIE-ID ::= 92

id-ReportingPeriodicity ProtocolIE-ID ::= 93

id-TNL-AvailableCapacityIndicator ProtocolIE-ID ::= 94

id-HW-CapacityIndicator ProtocolIE-ID ::= 95

id-RedundantCommonNetworkInstance ProtocolIE-ID ::= 96

id-redundant-nG-UL-UP-TNL-Information ProtocolIE-ID ::= 97

id-redundant-nG-DL-UP-TNL-Information ProtocolIE-ID ::= 98

id-RedundantQosFlowIndicator ProtocolIE-ID ::= 99

id-TSCTrafficCharacteristics ProtocolIE-ID ::= 100

id-CNPacketDelayBudgetDownlink ProtocolIE-ID ::= 101

id-CNPacketDelayBudgetUplink ProtocolIE-ID ::= 102

id-ExtendedPacketDelayBudget ProtocolIE-ID ::= 103

id-AdditionalPDCPduplicationInformation ProtocolIE-ID ::= 104

id-RedundantPDUSessionInformation ProtocolIE-ID ::= 105

id-RedundantPDUSessionInformation-used ProtocolIE-ID ::= 106

id-QoS-Mapping-Information ProtocolIE-ID ::= 107

id-DLUPTNLAddressToUpdateList ProtocolIE-ID ::= 108

id-ULUPTNLAddressToUpdateList ProtocolIE-ID ::= 109

id-NPNSupportInfo ProtocolIE-ID ::= 110

id-NPNContextInfo ProtocolIE-ID ::= 111

id-MDTConfiguration ProtocolIE-ID ::= 112

id-ManagementBasedMDTPLMNList ProtocolIE-ID ::= 113

id-TraceCollectionEntityIPAddress ProtocolIE-ID ::= 114

id-PrivacyIndicator ProtocolIE-ID ::= 115

id-TraceCollectionEntityURI ProtocolIE-ID ::= 116

id-URIaddress ProtocolIE-ID ::= 117

id-EHC-Parameters ProtocolIE-ID ::= 118

id-DRBs-Subject-To-Early-Forwarding-List ProtocolIE-ID ::= 119

id-DAPSRequestInfo ProtocolIE-ID ::= 120

id-CHOInitiation ProtocolIE-ID ::= 121

id-EarlyForwardingCOUNTReq ProtocolIE-ID ::= 122

id-EarlyForwardingCOUNTInfo ProtocolIE-ID ::= 123

id-AlternativeQoSParaSetList ProtocolIE-ID ::= 124

 id-ExtendedSliceSupportList ProtocolIE-ID ::= 125

id-MCG-OfferedGBRQoSFlowInfo ProtocolIE-ID ::= 126

id-Number-of-tunnels ProtocolIE-ID ::= 127

id-DRB-Measurement-Results-Information-List ProtocolIE-ID ::= 128

id-Extended-GNB-CU-CP-Name ProtocolIE-ID ::= 129

id-Extended-GNB-CU-UP-Name ProtocolIE-ID ::= 130

id-DataForwardingtoE-UTRANInformationList ProtocolIE-ID ::= 131

id-QosMonitoringReportingFrequency ProtocolIE-ID ::= 132

id-QoSMonitoringDisabled ProtocolIE-ID ::= 133

id-AdditionalHandoverInfo ProtocolIE-ID ::= 134

id-Extended-NR-CGI-Support-List ProtocolIE-ID ::= 135

id-DataForwardingtoNG-RANQoSFlowInformationList ProtocolIE-ID ::= 136

id-MaxCIDEHCDL ProtocolIE-ID ::= 137

id-ignoreMappingRuleIndication ProtocolIE-ID ::= 138

id-DirectForwardingPathAvailability ProtocolIE-ID ::= 139

id-EarlyDataForwardingIndicator ProtocolIE-ID ::= 140

id-QoSFlowsDRBRemapping ProtocolIE-ID ::= 141

id-DataForwardingSourceIPAddress ProtocolIE-ID ::= 142

id-SecurityIndicationModify ProtocolIE-ID ::= 143

id-IAB-Donor-CU-UPPSKInfo ProtocolIE-ID ::= 144

id-DiscardTimerExtended ProtocolIE-ID ::= 177

id-Handover-With-Full-Configuration ProtocolIE-ID ::= 1xx

END

-- ASN1STOP