**3GPP TSG-RAN WG3 #119bis-e R3-231915**

**Online, 17th – 26th April 2023**

**Title: [DRAFT]** LS for clarification on the maximum length of Routing ID

**Response to:** -

**Release:** Rel-16

**Work Items:** NR\_pos-Core

**Source:** NTTDOCOMO, INC. [to be RAN3]

**To:** SA2, CT4

**CC:**

**Contact Person:** Tianyang Min

#### Name:

E-mail Address: tianyang.min.ex@nttdocomo.com

**Attachment:** R3-231913, R3-231914

**1. Overall Description:**

Regarding LMF *Routing ID* IE in the NRPPa transport messages defined in TS 38.413, RAN3 has agreed to the attached CRs which clarify that the maximum length of the *Routing ID* IE is 16 octets, referring to the value of NfInstanceId defined in TS 29.571 (and IETF RFC 4122).

**2. Actions:**

**To SA2 and CT4**

**ACTION:** RAN3 respectfully asks SA2 and CT4 to take the above information into account.

**3. Date of Next RAN WG Meetings:**

TSG-RAN3 Meeting #120 May 22 to May 26, 2023 Incheon

TSG-RAN3 Meeting #121 August 21 to August 25, 2023 Toulouse