**3GPP TSG-RAN WG3 Meeting #120 R3-23xxxx**

Incheon, Korea, 22nd – 26th May, 2023

**Title:** (TP for NR\_mobile\_IAB BL CR for TS 38.413) additional ULI

**Source:** Huawei

**Agenda item:** 13.5

**Document Type:** Other

# Introduction

This TP is provided per following CB:

**CB: IAB2\_Others:**

* **Check if CRs can be agreed**
* **Check if LS can be agreed**

**(Moderator – Xiaomi)**

# Annex: Text Proposal for TS 38.413

-------------------------------------------------Start of change-----------------------------------------------------------

#### 9.3.1.16 User Location Information

This IE is used to provide location information of the UE.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| CHOICE *User Location Information* | M |  |  |  | - |  |
| >*E-UTRA user location information* |  |  |  |  |  |  |
| >>E-UTRA CGI | M |  | 9.3.1.9 |  | - |  |
| >>TAI | M |  | 9.3.3.11 |  | - |  |
| >>Age of Location | O |  | Time Stamp9.3.1.75 | Indicates the UTC time when the location information was generated. | - |  |
| >>PSCell Information | O |  | NG-RAN CGI9.3.1.73 |  | YES | ignore |
| >*NR user location information* |  |  |  |  |  |  |
| >>NR CGI | M |  | 9.3.1.7 |  | - |  |
| >>TAI | M |  | 9.3.3.11 | This IE is ignored if the *NR NTN TAI Information* IE is present. | - |  |
| >>Age of Location | O |  | Time Stamp9.3.1.75 | Indicates the UTC time when the location information was generated. | - |  |
| >>PSCell Information | O |  | NG-RAN CGI9.3.1.73 |  | YES | ignore |
| >>NID | O |  | 9.3.3.42 |  | YES | reject |
| >>NR NTN TAI Information | O |  | 9.3.3.53 |  | YES | ignore |
| >> IAB-MT User Location Information | O |  | 9.3.1.x | Indicates the user location information of IAB-MT, which is co-located with the UE’s serving IAB-DU. | - |  |
| >*N3IWF user location information* |  |  |  |  |  |  |
| >>IP Address | M |  | Transport Layer Address 9.3.2.4 | UE's local IP address used to reach the N3IWF | - |  |
| >>Port Number | O |  | OCTET STRING(SIZE(2)) | UDP or TCP source port number if NAT is detected. | - |  |
| >>TAI | O |  | 9.3.3.11 |  | YES | ignore |
| >*TNGF user location information* |  |  |  |  | YES | ignore |
| >>TNAP ID | M |  |  OCTET STRING | TNAP Identifier used to identify the TNAP. Details in TS 29.571 [35]. | - |  |
| >>IP Address | M |  | Transport Layer Address 9.3.2.4 | UE's local IP address used to reach the TNGF. | - |  |
| >>Port Number | O |  | OCTET STRING(SIZE(2)) | UDP or TCP source port number if NAT is detected. | - |  |
| >>TAI | O |  | 9.3.3.11 |  | YES | ignore |
| >*TWIF user location information* |  |  |  |  | YES | ignore |
| >>TWAP ID | M |  | OCTET STRING | TWAP Identifier used to identify the TWAP. Details in TS 29.571 [35]. | - |  |
| >>IP Address | M |  | Transport Layer Address 9.3.2.4 | Non-5G-Capable over WLAN device's local IP address used to reach the TWIF. | - |  |
| >>Port Number | O |  | OCTET STRING(SIZE(2)) | UDP or TCP source port number if NAT is detected. | - |  |
| >>TAI | O |  | 9.3.3.11 |  | YES | ignore |
| >*W-AGF user location information* |  |  |  | Indicates the location information via wireline access as specified in TS 23.316 [34]. | YES | ignore |
| >>W-AGF user location information | M |  | 9.3.1.164 |  | - |  |

-------------------------------------------------Next change-----------------------------------------------------------

#### 9.3.1.x IAB-MT User Location Information

This IE contains the NR CGI and the TAI for the co-located IAB-MT of the UE’s serving IAB-DU.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| IE/Group Name | Presence | Range | IE type and reference | Semantics description |
| NR CGI | M |  | 9.3.1.7 | The NR CGI of the cell, which is the serving cell of the IAB-MT co-located with the UE’s serving IAB-DU  |
| TAI | M |  | 9.3.3.11 | The TAI supported by the cell, which is the serving cell of the IAB-MT co-located with the UE’s serving IAB-DU |

-------------------------------------------------Next change-----------------------------------------------------------

### 9.4.5 Information Element Definitions

-- ASN1START

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Information Element Definitions

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

NGAP-IEs {

itu-t (0) identified-organization (4) etsi (0) mobileDomain (0)

ngran-Access (22) modules (3) ngap (1) version1 (1) ngap-IEs (2) }

DEFINITIONS AUTOMATIC TAGS ::=

BEGIN

IMPORTS

 id-AdditionalDLForwardingUPTNLInformation,

 id-AdditionalULForwardingUPTNLInformation,

 id-AdditionalDLQosFlowPerTNLInformation,

 id-AdditionalDLUPTNLInformationForHOList,

 id-AdditionalNGU-UP-TNLInformation,

 id-AdditionalRedundantDL-NGU-UP-TNLInformation,

 id-AdditionalRedundantDLQosFlowPerTNLInformation,

 id-AdditionalRedundantNGU-UP-TNLInformation,

 id-AdditionalRedundantUL-NGU-UP-TNLInformation,

 id-AdditionalUL-NGU-UP-TNLInformation,

 id-AlternativeQoSParaSetList,

 id-BurstArrivalTimeDownlink,

 id-Cause,

 id-CNPacketDelayBudgetDL,

 id-CNPacketDelayBudgetUL,

 id-CNTypeRestrictionsForEquivalent,

 id-CNTypeRestrictionsForServing,

 id-CommonNetworkInstance,

 id-ConfiguredTACIndication,

 id-CurrentQoSParaSetIndex,

 id-DAPSRequestInfo,

 id-DAPSResponseInfoList,

 id-DataForwardingNotPossible,

 id-DataForwardingResponseERABList,

 id-DirectForwardingPathAvailability,

 id-DL-NGU-UP-TNLInformation,

 id-EndpointIPAddressAndPort,

 id-EnergySavingIndication,

 id-ExtendedPacketDelayBudget,

 id-ExtendedRATRestrictionInformation,

 id-ExtendedReportIntervalMDT,

 id-ExtendedSliceSupportList,

 id-ExtendedTAISliceSupportList,

 id-ExtendedUEIdentityIndexValue,

 id-EUTRA-PagingeDRXInformation,

 id-GlobalCable-ID,

 id-GlobalRANNodeID,

 id-GlobalTNGF-ID,

 id-GlobalTWIF-ID,

 id-GlobalW-AGF-ID,

 id-GUAMIType,

 id-IncludeBeamMeasurementsIndication,

 id-IntersystemSONInformationRequest,

 id-IntersystemSONInformationReply,

 id-IntersystemResourceStatusUpdate,

 id-LastEUTRAN-PLMNIdentity,

 id-LastVisitedPSCellList,

 id-LocationReportingAdditionalInfo,

 id-M4ReportAmount,

 id-M5ReportAmount,

 id-M6ReportAmount,

 id-ExcessPacketDelayThresholdConfiguration,

 id-M7ReportAmount,

 id-MaximumIntegrityProtectedDataRate-DL,

 id-MBS-AreaSessionID,

 id-MBS-QoSFlowsToBeSetupList,

 id-MBS-QoSFlowsToBeSetupModList,

 id-MBS-QoSFlowToReleaseList,

 id-MBS-ServiceArea,

 id-MBS-SessionFSAIDList,

 id-MBS-SessionID,

 id-MBS-ActiveSessionInformation-SourcetoTargetList,

 id-MBS-ActiveSessionInformation-TargettoSourceList,

 id-MBS-SessionTNLInfo5GC,

 id-MBS-SupportIndicator,

 id-MBSSessionFailedtoSetupList,

 id-MBSSessionFailedtoSetuporModifyList,

 id-MBSSessionSetupResponseList,

 id-MBSSessionSetuporModifyResponseList,

 id-MBSSessionToReleaseList,

 id-MBSSessionSetupRequestList,

 id-MBSSessionSetuporModifyRequestList,

 id-MDTConfiguration,

 id-MicoAllPLMN,

 id-NetworkInstance,

 id-NGAPIESupportInformationRequestList,

 id-NGAPIESupportInformationResponseList,

 id-NID,

 id-NR-CGI,

 id-NRNTNTAIInformation,

 id-NPN-MobilityInformation,

 id-NPN-PagingAssistanceInformation,

 id-NPN-Support,

 id-NR-PagingeDRXInformation,

 id-OldAssociatedQosFlowList-ULendmarkerexpected,

 id-OnboardingSupport,

 id-PagingAssisDataforCEcapabUE,

 id-PagingCauseIndicationForVoiceService,

 id-PDUSessionAggregateMaximumBitRate,

 id-PduSessionExpectedUEActivityBehaviour,

 id-PDUSessionPairID,

 id-PDUSessionResourceFailedToSetupListCxtFail,

 id-PDUSessionResourceReleaseResponseTransfer,

 id-PDUSessionType,

 id-PEIPSassistanceInformation,

 id-PSCellInformation,

 id-QMCConfigInfo,

 id-QosFlowAddOrModifyRequestList,

 id-QosFlowFailedToSetupList,

 id-QosFlowFeedbackList,

 id-QosFlowParametersList,

 id-QosFlowSetupRequestList,

 id-QosFlowToReleaseList,

 id-QosMonitoringRequest,

 id-QosMonitoringReportingFrequency,

 id-SuccessfulHandoverReportList,

 id-UEContextReferenceAtSource,

 id-RAT-Information,

 id-RedundantCommonNetworkInstance,

 id-RedundantDL-NGU-TNLInformationReused,

 id-RedundantDL-NGU-UP-TNLInformation,

 id-RedundantDLQosFlowPerTNLInformation,

 id-RedundantPDUSessionInformation,

 id-RedundantQosFlowIndicator,

 id-RedundantUL-NGU-UP-TNLInformation,

 id-SCTP-TLAs,

 id-SecondaryRATUsageInformation,

 id-SecurityIndication,

 id-SecurityResult,

 id-SgNB-UE-X2AP-ID,

 id-S-NSSAI,

 id-SONInformationReport,

 id-SourceNodeID,

 id-SourceNodeTNLAddrInfo,

 id-SourceTNLAddrInfo,

 id-SurvivalTime,

 id-TNLAssociationTransportLayerAddressNGRAN,

 id-TAINSAGSupportList,

 id-TargetHomeENB-ID,

 id-TargetRNC-ID,

 id-TraceCollectionEntityURI,

 id-TSCTrafficCharacteristics,

 id-UEHistoryInformationFromTheUE,

 id-UERadioCapabilityForPaging,

 id-UERadioCapabilityForPagingOfNB-IoT,

 id-UL-NGU-UP-TNLInformation,

 id-UL-NGU-UP-TNLModifyList,

 id-ULForwarding,

 id-ULForwardingUP-TNLInformation,

 id-UsedRSNInformation,

 id-UserLocationInformationTNGF,

 id-UserLocationInformationTWIF,

 id-UserLocationInformationW-AGF,

 id-EarlyMeasurement,

 id-BeamMeasurementsReportConfiguration,

 id-TAI,

 id-HFCNode-ID-new,

 id-GlobalCable-ID-new,

 id-IAB-MTUserLocationInformation,

 maxnoofAllowedAreas,

 maxnoofAllowedCAGsperPLMN,

 maxnoofAllowedS-NSSAIs,

 maxnoofBluetoothName,

 maxnoofBPLMNs,

 maxnoofCAGSperCell,

 maxnoofCandidateCells,

 maxnoofCellIDforMDT,

 maxnoofCellIDforQMC,

 maxnoofCellIDforWarning,

 maxnoofCellinAoI,

 maxnoofCellinEAI,

 maxnoofCellsforMBS,

 maxnoofCellsingNB,

 maxnoofCellsinngeNB,

 maxnoofCellsinNGRANNode,

 maxnoofCellinTAI,

 maxnoofCellsinUEHistoryInfo,

 maxnoofCellsUEMovingTrajectory,

 maxnoofDRBs,

 maxnoofEmergencyAreaID,

 maxnoofEAIforRestart,

 maxnoofEPLMNs,

 maxnoofEPLMNsPlusOne,

 maxnoofE-RABs,

 maxnoofErrors,

 maxnoofExtSliceItems,

 maxnoofForbTACs,

 maxnoofFreqforMDT,

 maxnoofMBSFSAs,

 maxnoofMBSQoSFlows,

 maxnoofMBSServiceAreaInformation,

 maxnoofMBSAreaSessionIDs,

 maxnoofMBSSessions,

 maxnoofMBSSessionsofUE,

 maxnoofMDTPLMNs,

 maxnoofMRBs,

 maxnoofMultiConnectivity,

 maxnoofMultiConnectivityMinusOne,

 maxnoofNeighPCIforMDT,

 maxnoofNGAPIESupportInfo,

 maxnoofNGConnectionsToReset,

 maxNRARFCN,

 maxnoofNRCellBands,

 maxnoofNSAGs,

 maxnoofPagingAreas,

 maxnoofPC5QoSFlows,

 maxnoofPDUSessions,

 maxnoofPLMNs,

 maxnoofPLMNforQMC,

 maxnoofQosFlows,

 maxnoofQosParaSets,

 maxnoofRANNodeinAoI,

 maxnoofRecommendedCells,

 maxnoofRecommendedRANNodes,

 maxnoofAoI,

 maxnoofPSCellsPerPrimaryCellinUEHistoryInfo,

 maxnoofReportedCells,

 maxnoofSensorName,

 maxnoofServedGUAMIs,

 maxnoofSliceItems,

 maxnoofSNSSAIforQMC,

 maxnoofSuccessfulHOReports,

 maxnoofTACs,

 maxnoofTACsinNTN,

 maxnoofTAforMDT,

 maxnoofTAforQMC,

 maxnoofTAIforInactive,

 maxnoofTAIforMBS,

 maxnoofTAIforPaging,

 maxnoofTAIforRestart,

 maxnoofTAIforWarning,

 maxnoofTAIinAoI,

 maxnoofTargetS-NSSAIs,

 maxnoofTimePeriods,

 maxnoofTNLAssociations,

 maxnoofUEAppLayerMeas,

 maxnoofUEsforPaging,

 maxnoofWLANName,

 maxnoofXnExtTLAs,

 maxnoofXnGTP-TLAs,

 maxnoofXnTLAs,

 maxnoofThresholdsForExcessPacketDelay

FROM NGAP-Constants

 Criticality,

 ProcedureCode,

 ProtocolIE-ID,

 TriggeringMessage

FROM NGAP-CommonDataTypes

 ProtocolExtensionContainer{},

 ProtocolIE-Container{},

 NGAP-PROTOCOL-EXTENSION,

 ProtocolIE-SingleContainer{},

 NGAP-PROTOCOL-IES

FROM NGAP-Containers;

-------------------------------------------------Next change-----------------------------------------------------------

-- I

IAB-Authorized ::= ENUMERATED {

 authorized,

 not-authorized,

 ...

}

IAB-MTUserLocationInformation ::= SEQUENCE {

 nRCGI NR-CGI,

 tAI TAI,

 iE-Extensions ProtocolExtensionContainer { { IAB-MTUserLocationInformation-ExtIEs} } OPTIONAL,

 ...

}

IAB-MTUserLocationInformation-ExtIEs F1AP-PROTOCOL-EXTENSION ::= {

 ...

}

IAB-Supported ::= ENUMERATED {

 true,

 ...

}

IABNodeIndication ::= ENUMERATED {

 true,

 ...

}

IMSVoiceSupportIndicator ::= ENUMERATED {

 supported,

 not-supported,

 ...

}

-------------------------------------------------Next change-----------------------------------------------------------

-- U

UserLocationInformation ::= CHOICE {

 userLocationInformationEUTRA UserLocationInformationEUTRA,

 userLocationInformationNR UserLocationInformationNR,

 userLocationInformationN3IWF UserLocationInformationN3IWF,

 choice-Extensions ProtocolIE-SingleContainer { {UserLocationInformation-ExtIEs} }

}

UserLocationInformation-ExtIEs NGAP-PROTOCOL-IES ::= {

 { ID id-UserLocationInformationTNGF CRITICALITY ignore TYPE UserLocationInformationTNGF PRESENCE mandatory }|

 { ID id-UserLocationInformationTWIF CRITICALITY ignore TYPE UserLocationInformationTWIF PRESENCE mandatory }|

 { ID id-UserLocationInformationW-AGF CRITICALITY ignore TYPE UserLocationInformationW-AGF PRESENCE mandatory },

 ...

}

UserLocationInformationEUTRA ::= SEQUENCE {

 eUTRA-CGI EUTRA-CGI,

 tAI TAI,

 timeStamp TimeStamp OPTIONAL,

 iE-Extensions ProtocolExtensionContainer { {UserLocationInformationEUTRA-ExtIEs} } OPTIONAL,

 ...

}

UserLocationInformationEUTRA-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {

 { ID id-PSCellInformation CRITICALITY ignore EXTENSION NGRAN-CGI PRESENCE optional},

 ...

}

UserLocationInformationN3IWF ::= SEQUENCE {

 iPAddress TransportLayerAddress,

 portNumber PortNumber,

 iE-Extensions ProtocolExtensionContainer { {UserLocationInformationN3IWF-ExtIEs} } OPTIONAL,

 ...

}

UserLocationInformationN3IWF-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {

 { ID id-TAI CRITICALITY ignore EXTENSION TAI PRESENCE optional },

 ...

}

UserLocationInformationTNGF ::= SEQUENCE {

 tNAP-ID TNAP-ID,

 iPAddress TransportLayerAddress,

 portNumber PortNumber OPTIONAL,

 iE-Extensions ProtocolExtensionContainer { {UserLocationInformationTNGF-ExtIEs} } OPTIONAL,

 ...

}

UserLocationInformationTNGF-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {

 { ID id-TAI CRITICALITY ignore EXTENSION TAI PRESENCE optional },

 ...

}

UserLocationInformationTWIF ::= SEQUENCE {

 tWAP-ID TWAP-ID,

 iPAddress TransportLayerAddress,

 portNumber PortNumber OPTIONAL,

 iE-Extensions ProtocolExtensionContainer { {UserLocationInformationTWIF-ExtIEs} } OPTIONAL,

 ...

}

UserLocationInformationTWIF-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {

 { ID id-TAI CRITICALITY ignore EXTENSION TAI PRESENCE optional },

 ...

}

UserLocationInformationW-AGF ::= CHOICE {

 globalLine-ID GlobalLine-ID,

 hFCNode-ID HFCNode-ID,

 choice-Extensions ProtocolIE-SingleContainer { { UserLocationInformationW-AGF-ExtIEs} }

}

UserLocationInformationW-AGF-ExtIEs NGAP-PROTOCOL-IES ::= {

 { ID id-GlobalCable-ID CRITICALITY ignore TYPE GlobalCable-ID PRESENCE mandatory }|

 { ID id-HFCNode-ID-new CRITICALITY ignore TYPE HFCNode-ID-new PRESENCE mandatory }|

 { ID id-GlobalCable-ID-new CRITICALITY ignore TYPE GlobalCable-ID-new PRESENCE mandatory },

 ...

}

UserLocationInformationNR ::= SEQUENCE {

 nR-CGI NR-CGI,

 tAI TAI,

 timeStamp TimeStamp OPTIONAL,

 iE-Extensions ProtocolExtensionContainer { {UserLocationInformationNR-ExtIEs} } OPTIONAL,

 ...

}

UserLocationInformationNR-ExtIEs NGAP-PROTOCOL-EXTENSION ::= {

 { ID id-PSCellInformation CRITICALITY ignore EXTENSION NGRAN-CGI PRESENCE optional }|

 { ID id-NID CRITICALITY reject EXTENSION NID PRESENCE optional }|

 { ID id-NRNTNTAIInformation CRITICALITY ignore EXTENSION NRNTNTAIInformation PRESENCE optional }|

 { ID id-IAB-MTUserLocationInformation CRITICALITY ignore EXTENSION IAB-MTUserLocationInformation PRESENCE optional },

 ...

}

-------------------------------------------------Next change-----------------------------------------------------------

### 9.4.7 Constant Definitions

>>>>>>>>>>>>>>>unchanged parts are skipped<<<<<<<<<<<<<<<

-- IEs

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

 id-AllowedNSSAI ProtocolIE-ID ::= 0

 id-AMFName ProtocolIE-ID ::= 1

 id-AMFOverloadResponse ProtocolIE-ID ::= 2

 id-AMFSetID ProtocolIE-ID ::= 3

 id-AMF-TNLAssociationFailedToSetupList ProtocolIE-ID ::= 4

 id-AMF-TNLAssociationSetupList ProtocolIE-ID ::= 5

 id-AMF-TNLAssociationToAddList ProtocolIE-ID ::= 6

 id-AMF-TNLAssociationToRemoveList ProtocolIE-ID ::= 7

 id-AMF-TNLAssociationToUpdateList ProtocolIE-ID ::= 8

 id-AMFTrafficLoadReductionIndication ProtocolIE-ID ::= 9

 id-AMF-UE-NGAP-ID ProtocolIE-ID ::= 10

 id-AssistanceDataForPaging ProtocolIE-ID ::= 11

 id-BroadcastCancelledAreaList ProtocolIE-ID ::= 12

 id-BroadcastCompletedAreaList ProtocolIE-ID ::= 13

 id-CancelAllWarningMessages ProtocolIE-ID ::= 14

 id-Cause ProtocolIE-ID ::= 15

 id-CellIDListForRestart ProtocolIE-ID ::= 16

 id-ConcurrentWarningMessageInd ProtocolIE-ID ::= 17

 id-CoreNetworkAssistanceInformationForInactive ProtocolIE-ID ::= 18

 id-CriticalityDiagnostics ProtocolIE-ID ::= 19

 id-DataCodingScheme ProtocolIE-ID ::= 20

 id-DefaultPagingDRX ProtocolIE-ID ::= 21

 id-DirectForwardingPathAvailability ProtocolIE-ID ::= 22

 id-EmergencyAreaIDListForRestart ProtocolIE-ID ::= 23

 id-EmergencyFallbackIndicator ProtocolIE-ID ::= 24

 id-EUTRA-CGI ProtocolIE-ID ::= 25

 id-FiveG-S-TMSI ProtocolIE-ID ::= 26

 id-GlobalRANNodeID ProtocolIE-ID ::= 27

 id-GUAMI ProtocolIE-ID ::= 28

 id-HandoverType ProtocolIE-ID ::= 29

 id-IMSVoiceSupportIndicator ProtocolIE-ID ::= 30

 id-IndexToRFSP ProtocolIE-ID ::= 31

 id-InfoOnRecommendedCellsAndRANNodesForPaging ProtocolIE-ID ::= 32

 id-LocationReportingRequestType ProtocolIE-ID ::= 33

 id-MaskedIMEISV ProtocolIE-ID ::= 34

 id-MessageIdentifier ProtocolIE-ID ::= 35

 id-MobilityRestrictionList ProtocolIE-ID ::= 36

 id-NASC ProtocolIE-ID ::= 37

 id-NAS-PDU ProtocolIE-ID ::= 38

 id-NASSecurityParametersFromNGRAN ProtocolIE-ID ::= 39

 id-NewAMF-UE-NGAP-ID ProtocolIE-ID ::= 40

 id-NewSecurityContextInd ProtocolIE-ID ::= 41

 id-NGAP-Message ProtocolIE-ID ::= 42

 id-NGRAN-CGI ProtocolIE-ID ::= 43

 id-NGRANTraceID ProtocolIE-ID ::= 44

 id-NR-CGI ProtocolIE-ID ::= 45

 id-NRPPa-PDU ProtocolIE-ID ::= 46

 id-NumberOfBroadcastsRequested ProtocolIE-ID ::= 47

 id-OldAMF ProtocolIE-ID ::= 48

 id-OverloadStartNSSAIList ProtocolIE-ID ::= 49

 id-PagingDRX ProtocolIE-ID ::= 50

 id-PagingOrigin ProtocolIE-ID ::= 51

 id-PagingPriority ProtocolIE-ID ::= 52

 id-PDUSessionResourceAdmittedList ProtocolIE-ID ::= 53

 id-PDUSessionResourceFailedToModifyListModRes ProtocolIE-ID ::= 54

 id-PDUSessionResourceFailedToSetupListCxtRes ProtocolIE-ID ::= 55

 id-PDUSessionResourceFailedToSetupListHOAck ProtocolIE-ID ::= 56

 id-PDUSessionResourceFailedToSetupListPSReq ProtocolIE-ID ::= 57

 id-PDUSessionResourceFailedToSetupListSURes ProtocolIE-ID ::= 58

 id-PDUSessionResourceHandoverList ProtocolIE-ID ::= 59

 id-PDUSessionResourceListCxtRelCpl ProtocolIE-ID ::= 60

 id-PDUSessionResourceListHORqd ProtocolIE-ID ::= 61

 id-PDUSessionResourceModifyListModCfm ProtocolIE-ID ::= 62

 id-PDUSessionResourceModifyListModInd ProtocolIE-ID ::= 63

 id-PDUSessionResourceModifyListModReq ProtocolIE-ID ::= 64

 id-PDUSessionResourceModifyListModRes ProtocolIE-ID ::= 65

 id-PDUSessionResourceNotifyList ProtocolIE-ID ::= 66

 id-PDUSessionResourceReleasedListNot ProtocolIE-ID ::= 67

 id-PDUSessionResourceReleasedListPSAck ProtocolIE-ID ::= 68

 id-PDUSessionResourceReleasedListPSFail ProtocolIE-ID ::= 69

 id-PDUSessionResourceReleasedListRelRes ProtocolIE-ID ::= 70

 id-PDUSessionResourceSetupListCxtReq ProtocolIE-ID ::= 71

 id-PDUSessionResourceSetupListCxtRes ProtocolIE-ID ::= 72

 id-PDUSessionResourceSetupListHOReq ProtocolIE-ID ::= 73

 id-PDUSessionResourceSetupListSUReq ProtocolIE-ID ::= 74

 id-PDUSessionResourceSetupListSURes ProtocolIE-ID ::= 75

 id-PDUSessionResourceToBeSwitchedDLList ProtocolIE-ID ::= 76

 id-PDUSessionResourceSwitchedList ProtocolIE-ID ::= 77

 id-PDUSessionResourceToReleaseListHOCmd ProtocolIE-ID ::= 78

 id-PDUSessionResourceToReleaseListRelCmd ProtocolIE-ID ::= 79

 id-PLMNSupportList ProtocolIE-ID ::= 80

 id-PWSFailedCellIDList ProtocolIE-ID ::= 81

 id-RANNodeName ProtocolIE-ID ::= 82

 id-RANPagingPriority ProtocolIE-ID ::= 83

 id-RANStatusTransfer-TransparentContainer ProtocolIE-ID ::= 84

 id-RAN-UE-NGAP-ID ProtocolIE-ID ::= 85

 id-RelativeAMFCapacity ProtocolIE-ID ::= 86

 id-RepetitionPeriod ProtocolIE-ID ::= 87

 id-ResetType ProtocolIE-ID ::= 88

 id-RoutingID ProtocolIE-ID ::= 89

 id-RRCEstablishmentCause ProtocolIE-ID ::= 90

 id-RRCInactiveTransitionReportRequest ProtocolIE-ID ::= 91

 id-RRCState ProtocolIE-ID ::= 92

 id-SecurityContext ProtocolIE-ID ::= 93

 id-SecurityKey ProtocolIE-ID ::= 94

 id-SerialNumber ProtocolIE-ID ::= 95

 id-ServedGUAMIList ProtocolIE-ID ::= 96

 id-SliceSupportList ProtocolIE-ID ::= 97

 id-SONConfigurationTransferDL ProtocolIE-ID ::= 98

 id-SONConfigurationTransferUL ProtocolIE-ID ::= 99

 id-SourceAMF-UE-NGAP-ID ProtocolIE-ID ::= 100

 id-SourceToTarget-TransparentContainer ProtocolIE-ID ::= 101

 id-SupportedTAList ProtocolIE-ID ::= 102

 id-TAIListForPaging ProtocolIE-ID ::= 103

 id-TAIListForRestart ProtocolIE-ID ::= 104

 id-TargetID ProtocolIE-ID ::= 105

 id-TargetToSource-TransparentContainer ProtocolIE-ID ::= 106

 id-TimeToWait ProtocolIE-ID ::= 107

 id-TraceActivation ProtocolIE-ID ::= 108

 id-TraceCollectionEntityIPAddress ProtocolIE-ID ::= 109

 id-UEAggregateMaximumBitRate ProtocolIE-ID ::= 110

 id-UE-associatedLogicalNG-connectionList ProtocolIE-ID ::= 111

 id-UEContextRequest ProtocolIE-ID ::= 112

 id-UE-NGAP-IDs ProtocolIE-ID ::= 114

 id-UEPagingIdentity ProtocolIE-ID ::= 115

 id-UEPresenceInAreaOfInterestList ProtocolIE-ID ::= 116

 id-UERadioCapability ProtocolIE-ID ::= 117

 id-UERadioCapabilityForPaging ProtocolIE-ID ::= 118

 id-UESecurityCapabilities ProtocolIE-ID ::= 119

 id-UnavailableGUAMIList ProtocolIE-ID ::= 120

 id-UserLocationInformation ProtocolIE-ID ::= 121

 id-WarningAreaList ProtocolIE-ID ::= 122

 id-WarningMessageContents ProtocolIE-ID ::= 123

 id-WarningSecurityInfo ProtocolIE-ID ::= 124

 id-WarningType ProtocolIE-ID ::= 125

 id-AdditionalUL-NGU-UP-TNLInformation ProtocolIE-ID ::= 126

 id-DataForwardingNotPossible ProtocolIE-ID ::= 127

 id-DL-NGU-UP-TNLInformation ProtocolIE-ID ::= 128

 id-NetworkInstance ProtocolIE-ID ::= 129

 id-PDUSessionAggregateMaximumBitRate ProtocolIE-ID ::= 130

 id-PDUSessionResourceFailedToModifyListModCfm ProtocolIE-ID ::= 131

 id-PDUSessionResourceFailedToSetupListCxtFail ProtocolIE-ID ::= 132

 id-PDUSessionResourceListCxtRelReq ProtocolIE-ID ::= 133

 id-PDUSessionType ProtocolIE-ID ::= 134

 id-QosFlowAddOrModifyRequestList ProtocolIE-ID ::= 135

 id-QosFlowSetupRequestList ProtocolIE-ID ::= 136

 id-QosFlowToReleaseList ProtocolIE-ID ::= 137

 id-SecurityIndication ProtocolIE-ID ::= 138

 id-UL-NGU-UP-TNLInformation ProtocolIE-ID ::= 139

 id-UL-NGU-UP-TNLModifyList ProtocolIE-ID ::= 140

 id-WarningAreaCoordinates ProtocolIE-ID ::= 141

 id-PDUSessionResourceSecondaryRATUsageList ProtocolIE-ID ::= 142

 id-HandoverFlag ProtocolIE-ID ::= 143

 id-SecondaryRATUsageInformation ProtocolIE-ID ::= 144

 id-PDUSessionResourceReleaseResponseTransfer ProtocolIE-ID ::= 145

 id-RedirectionVoiceFallback ProtocolIE-ID ::= 146

 id-UERetentionInformation ProtocolIE-ID ::= 147

 id-S-NSSAI ProtocolIE-ID ::= 148

 id-PSCellInformation ProtocolIE-ID ::= 149

 id-LastEUTRAN-PLMNIdentity ProtocolIE-ID ::= 150

 id-MaximumIntegrityProtectedDataRate-DL ProtocolIE-ID ::= 151

 id-AdditionalDLForwardingUPTNLInformation ProtocolIE-ID ::= 152

 id-AdditionalDLUPTNLInformationForHOList ProtocolIE-ID ::= 153

 id-AdditionalNGU-UP-TNLInformation ProtocolIE-ID ::= 154

 id-AdditionalDLQosFlowPerTNLInformation ProtocolIE-ID ::= 155

 id-SecurityResult ProtocolIE-ID ::= 156

 id-ENDC-SONConfigurationTransferDL ProtocolIE-ID ::= 157

 id-ENDC-SONConfigurationTransferUL ProtocolIE-ID ::= 158

 id-OldAssociatedQosFlowList-ULendmarkerexpected ProtocolIE-ID ::= 159

 id-CNTypeRestrictionsForEquivalent ProtocolIE-ID ::= 160

 id-CNTypeRestrictionsForServing ProtocolIE-ID ::= 161

 id-NewGUAMI ProtocolIE-ID ::= 162

 id-ULForwarding ProtocolIE-ID ::= 163

 id-ULForwardingUP-TNLInformation ProtocolIE-ID ::= 164

 id-CNAssistedRANTuning ProtocolIE-ID ::= 165

 id-CommonNetworkInstance ProtocolIE-ID ::= 166

 id-NGRAN-TNLAssociationToRemoveList ProtocolIE-ID ::= 167

 id-TNLAssociationTransportLayerAddressNGRAN ProtocolIE-ID ::= 168

 id-EndpointIPAddressAndPort ProtocolIE-ID ::= 169

 id-LocationReportingAdditionalInfo ProtocolIE-ID ::= 170

 id-SourceToTarget-AMFInformationReroute ProtocolIE-ID ::= 171

 id-AdditionalULForwardingUPTNLInformation ProtocolIE-ID ::= 172

 id-SCTP-TLAs ProtocolIE-ID ::= 173

 id-SelectedPLMNIdentity ProtocolIE-ID ::= 174

 id-RIMInformationTransfer ProtocolIE-ID ::= 175

 id-GUAMIType ProtocolIE-ID ::= 176

 id-SRVCCOperationPossible ProtocolIE-ID ::= 177

 id-TargetRNC-ID ProtocolIE-ID ::= 178

 id-RAT-Information ProtocolIE-ID ::= 179

 id-ExtendedRATRestrictionInformation ProtocolIE-ID ::= 180

 id-QosMonitoringRequest ProtocolIE-ID ::= 181

 id-SgNB-UE-X2AP-ID ProtocolIE-ID ::= 182

 id-AdditionalRedundantDL-NGU-UP-TNLInformation ProtocolIE-ID ::= 183

 id-AdditionalRedundantDLQosFlowPerTNLInformation ProtocolIE-ID ::= 184

 id-AdditionalRedundantNGU-UP-TNLInformation ProtocolIE-ID ::= 185

 id-AdditionalRedundantUL-NGU-UP-TNLInformation ProtocolIE-ID ::= 186

 id-CNPacketDelayBudgetDL ProtocolIE-ID ::= 187

 id-CNPacketDelayBudgetUL ProtocolIE-ID ::= 188

 id-ExtendedPacketDelayBudget ProtocolIE-ID ::= 189

 id-RedundantCommonNetworkInstance ProtocolIE-ID ::= 190

 id-RedundantDL-NGU-TNLInformationReused ProtocolIE-ID ::= 191

 id-RedundantDL-NGU-UP-TNLInformation ProtocolIE-ID ::= 192

 id-RedundantDLQosFlowPerTNLInformation ProtocolIE-ID ::= 193

 id-RedundantQosFlowIndicator ProtocolIE-ID ::= 194

 id-RedundantUL-NGU-UP-TNLInformation ProtocolIE-ID ::= 195

 id-TSCTrafficCharacteristics ProtocolIE-ID ::= 196

 id-RedundantPDUSessionInformation ProtocolIE-ID ::= 197

 id-UsedRSNInformation ProtocolIE-ID ::= 198

 id-IAB-Authorized ProtocolIE-ID ::= 199

 id-IAB-Supported ProtocolIE-ID ::= 200

 id-IABNodeIndication ProtocolIE-ID ::= 201

 id-NB-IoT-PagingDRX ProtocolIE-ID ::= 202

 id-NB-IoT-Paging-eDRXInfo ProtocolIE-ID ::= 203

 id-NB-IoT-DefaultPagingDRX ProtocolIE-ID ::= 204

 id-Enhanced-CoverageRestriction ProtocolIE-ID ::= 205

 id-Extended-ConnectedTime ProtocolIE-ID ::= 206

 id-PagingAssisDataforCEcapabUE ProtocolIE-ID ::= 207

 id-WUS-Assistance-Information ProtocolIE-ID ::= 208

 id-UE-DifferentiationInfo ProtocolIE-ID ::= 209

 id-NB-IoT-UEPriority ProtocolIE-ID ::= 210

 id-UL-CP-SecurityInformation ProtocolIE-ID ::= 211

 id-DL-CP-SecurityInformation ProtocolIE-ID ::= 212

 id-TAI ProtocolIE-ID ::= 213

 id-UERadioCapabilityForPagingOfNB-IoT ProtocolIE-ID ::= 214

 id-LTEV2XServicesAuthorized ProtocolIE-ID ::= 215

 id-NRV2XServicesAuthorized ProtocolIE-ID ::= 216

 id-LTEUESidelinkAggregateMaximumBitrate ProtocolIE-ID ::= 217

 id-NRUESidelinkAggregateMaximumBitrate ProtocolIE-ID ::= 218

 id-PC5QoSParameters ProtocolIE-ID ::= 219

 id-AlternativeQoSParaSetList ProtocolIE-ID ::= 220

 id-CurrentQoSParaSetIndex ProtocolIE-ID ::= 221

 id-CEmodeBrestricted ProtocolIE-ID ::= 222

 id-EUTRA-PagingeDRXInformation ProtocolIE-ID ::= 223

 id-CEmodeBSupport-Indicator ProtocolIE-ID ::= 224

 id-LTEM-Indication ProtocolIE-ID ::= 225

 id-EndIndication ProtocolIE-ID ::= 226

 id-EDT-Session ProtocolIE-ID ::= 227

 id-UECapabilityInfoRequest ProtocolIE-ID ::= 228

 id-PDUSessionResourceFailedToResumeListRESReq ProtocolIE-ID ::= 229

 id-PDUSessionResourceFailedToResumeListRESRes ProtocolIE-ID ::= 230

 id-PDUSessionResourceSuspendListSUSReq ProtocolIE-ID ::= 231

 id-PDUSessionResourceResumeListRESReq ProtocolIE-ID ::= 232

 id-PDUSessionResourceResumeListRESRes ProtocolIE-ID ::= 233

 id-UE-UP-CIoT-Support ProtocolIE-ID ::= 234

 id-Suspend-Request-Indication ProtocolIE-ID ::= 235

 id-Suspend-Response-Indication ProtocolIE-ID ::= 236

 id-RRC-Resume-Cause ProtocolIE-ID ::= 237

 id-RGLevelWirelineAccessCharacteristics ProtocolIE-ID ::= 238

 id-W-AGFIdentityInformation ProtocolIE-ID ::= 239

 id-GlobalTNGF-ID ProtocolIE-ID ::= 240

 id-GlobalTWIF-ID ProtocolIE-ID ::= 241

 id-GlobalW-AGF-ID ProtocolIE-ID ::= 242

 id-UserLocationInformationW-AGF ProtocolIE-ID ::= 243

 id-UserLocationInformationTNGF ProtocolIE-ID ::= 244

 id-AuthenticatedIndication ProtocolIE-ID ::= 245

 id-TNGFIdentityInformation ProtocolIE-ID ::= 246

 id-TWIFIdentityInformation ProtocolIE-ID ::= 247

 id-UserLocationInformationTWIF ProtocolIE-ID ::= 248

 id-DataForwardingResponseERABList ProtocolIE-ID ::= 249

 id-IntersystemSONConfigurationTransferDL ProtocolIE-ID ::= 250

 id-IntersystemSONConfigurationTransferUL ProtocolIE-ID ::= 251

 id-SONInformationReport ProtocolIE-ID ::= 252

 id-UEHistoryInformationFromTheUE ProtocolIE-ID ::= 253

 id-ManagementBasedMDTPLMNList ProtocolIE-ID ::= 254

 id-MDTConfiguration ProtocolIE-ID ::= 255

 id-PrivacyIndicator ProtocolIE-ID ::= 256

 id-TraceCollectionEntityURI ProtocolIE-ID ::= 257

 id-NPN-Support ProtocolIE-ID ::= 258

 id-NPN-AccessInformation ProtocolIE-ID ::= 259

 id-NPN-PagingAssistanceInformation ProtocolIE-ID ::= 260

 id-NPN-MobilityInformation ProtocolIE-ID ::= 261

 id-TargettoSource-Failure-TransparentContainer ProtocolIE-ID ::= 262

 id-NID ProtocolIE-ID ::= 263

 id-UERadioCapabilityID ProtocolIE-ID ::= 264

 id-UERadioCapability-EUTRA-Format ProtocolIE-ID ::= 265

 id-DAPSRequestInfo ProtocolIE-ID ::= 266

 id-DAPSResponseInfoList ProtocolIE-ID ::= 267

 id-EarlyStatusTransfer-TransparentContainer ProtocolIE-ID ::= 268

 id-NotifySourceNGRANNode ProtocolIE-ID ::= 269

 id-ExtendedSliceSupportList ProtocolIE-ID ::= 270

 id-ExtendedTAISliceSupportList ProtocolIE-ID ::= 271

 id-ConfiguredTACIndication ProtocolIE-ID ::= 272

 id-Extended-RANNodeName ProtocolIE-ID ::= 273

 id-Extended-AMFName ProtocolIE-ID ::= 274

 id-GlobalCable-ID ProtocolIE-ID ::= 275

 id-QosMonitoringReportingFrequency ProtocolIE-ID ::= 276

 id-QosFlowParametersList ProtocolIE-ID ::= 277

 id-QosFlowFeedbackList ProtocolIE-ID ::= 278

 id-BurstArrivalTimeDownlink ProtocolIE-ID ::= 279

 id-ExtendedUEIdentityIndexValue ProtocolIE-ID ::= 280

 id-PduSessionExpectedUEActivityBehaviour ProtocolIE-ID ::= 281

 id-MicoAllPLMN ProtocolIE-ID ::= 282

 id-QosFlowFailedToSetupList ProtocolIE-ID ::= 283

 id-SourceTNLAddrInfo ProtocolIE-ID ::= 284

 id-ExtendedReportIntervalMDT ProtocolIE-ID ::= 285

 id-SourceNodeID ProtocolIE-ID ::= 286

 id-NRNTNTAIInformation ProtocolIE-ID ::= 287

 id-UEContextReferenceAtSource ProtocolIE-ID ::= 288

 id-LastVisitedPSCellList ProtocolIE-ID ::= 289

 id-IntersystemSONInformationRequest ProtocolIE-ID ::= 290

 id-IntersystemSONInformationReply ProtocolIE-ID ::= 291

 id-EnergySavingIndication ProtocolIE-ID ::= 292

 id-IntersystemResourceStatusUpdate ProtocolIE-ID ::= 293

 id-SuccessfulHandoverReportList ProtocolIE-ID ::= 294

 id-MBS-AreaSessionID ProtocolIE-ID ::= 295

 id-MBS-QoSFlowsToBeSetupList ProtocolIE-ID ::= 296

 id-MBS-QoSFlowsToBeSetupModList ProtocolIE-ID ::= 297

 id-MBS-ServiceArea ProtocolIE-ID ::= 298

 id-MBS-SessionID ProtocolIE-ID ::= 299

 id-MBS-DistributionReleaseRequestTransfer ProtocolIE-ID ::= 300

 id-MBS-DistributionSetupRequestTransfer ProtocolIE-ID ::= 301

 id-MBS-DistributionSetupResponseTransfer ProtocolIE-ID ::= 302

 id-MBS-DistributionSetupUnsuccessfulTransfer ProtocolIE-ID ::= 303

 id-MulticastSessionActivationRequestTransfer ProtocolIE-ID ::= 304

 id-MulticastSessionDeactivationRequestTransfer ProtocolIE-ID ::= 305

 id-MulticastSessionUpdateRequestTransfer ProtocolIE-ID ::= 306

 id-MulticastGroupPagingAreaList ProtocolIE-ID ::= 307

 id-MBS-SupportIndicator ProtocolIE-ID ::= 309

 id-MBSSessionFailedtoSetupList ProtocolIE-ID ::= 310

 id-MBSSessionFailedtoSetuporModifyList ProtocolIE-ID ::= 311

 id-MBSSessionSetupResponseList ProtocolIE-ID ::= 312

 id-MBSSessionSetuporModifyResponseList ProtocolIE-ID ::= 313

 id-MBSSessionSetupFailureTransfer ProtocolIE-ID ::= 314

 id-MBSSessionSetupRequestTransfer ProtocolIE-ID ::= 315

 id-MBSSessionSetupResponseTransfer ProtocolIE-ID ::= 316

 id-MBSSessionToReleaseList ProtocolIE-ID ::= 317

 id-MBSSessionSetupRequestList ProtocolIE-ID ::= 318

 id-MBSSessionSetuporModifyRequestList ProtocolIE-ID ::= 319

 id-MBS-ActiveSessionInformation-SourcetoTargetList ProtocolIE-ID ::= 323

 id-MBS-ActiveSessionInformation-TargettoSourceList ProtocolIE-ID ::= 324

 id-OnboardingSupport ProtocolIE-ID ::= 325

 id-TimeSyncAssistanceInfo ProtocolIE-ID ::= 326

 id-SurvivalTime ProtocolIE-ID ::= 327

 id-QMCConfigInfo ProtocolIE-ID ::= 328

 id-QMCDeactivation ProtocolIE-ID ::= 329

 id-PDUSessionPairID ProtocolIE-ID ::= 331

 id-NR-PagingeDRXInformation ProtocolIE-ID ::= 332

 id-RedCapIndication ProtocolIE-ID ::= 333

 id-TargetNSSAIInformation ProtocolIE-ID ::= 334

 id-UESliceMaximumBitRateList ProtocolIE-ID ::= 335

 id-M4ReportAmount ProtocolIE-ID ::= 336

 id-M5ReportAmount ProtocolIE-ID ::= 337

 id-M6ReportAmount ProtocolIE-ID ::= 338

 id-M7ReportAmount ProtocolIE-ID ::= 339

 id-IncludeBeamMeasurementsIndication ProtocolIE-ID ::= 340

 id-ExcessPacketDelayThresholdConfiguration ProtocolIE-ID ::= 341

 id-PagingCause ProtocolIE-ID ::= 342

 id-PagingCauseIndicationForVoiceService ProtocolIE-ID ::= 343

 id-PEIPSassistanceInformation ProtocolIE-ID ::= 344

 id-FiveG-ProSeAuthorized ProtocolIE-ID ::= 345

 id-FiveG-ProSeUEPC5AggregateMaximumBitRate ProtocolIE-ID ::= 346

 id-FiveG-ProSePC5QoSParameters ProtocolIE-ID ::= 347

 id-MBSSessionModificationFailureTransfer ProtocolIE-ID ::= 348

 id-MBSSessionModificationRequestTransfer ProtocolIE-ID ::= 349

 id-MBSSessionModificationResponseTransfer ProtocolIE-ID ::= 350

 id-MBS-QoSFlowToReleaseList ProtocolIE-ID ::= 351

 id-MBS-SessionTNLInfo5GC ProtocolIE-ID ::= 352

 id-TAINSAGSupportList ProtocolIE-ID ::= 353

 id-SourceNodeTNLAddrInfo ProtocolIE-ID ::= 354

 id-NGAPIESupportInformationRequestList ProtocolIE-ID ::= 355

 id-NGAPIESupportInformationResponseList ProtocolIE-ID ::= 356

 id-MBS-SessionFSAIDList ProtocolIE-ID ::= 357

 id-MBSSessionReleaseResponseTransfer ProtocolIE-ID ::= 358

 id-ManagementBasedMDTPLMNModificationList ProtocolIE-ID ::= 359

 id-EarlyMeasurement ProtocolIE-ID ::= 360

 id-BeamMeasurementsReportConfiguration ProtocolIE-ID ::= 361

 id-HFCNode-ID-new ProtocolIE-ID ::= 362

 id-GlobalCable-ID-new ProtocolIE-ID ::= 363

 id-TargetHomeENB-ID ProtocolIE-ID ::= 364

 id-IAB-MTUserLocationInformation ProtocolIE-ID ::= xxx

END

-- ASN1STOP

-------------------------------------------------End of change-----------------------------------------------------------