**3GPP TSG-RAN WG3 Meeting #121 R3-234608**

**Toulouse, France, 21 – 25 Aug, 2023**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  | **38.423** | **CR** | **1076** | **rev** | **1** | **Current version:** | 16.14.0 |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **x** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Correction of Additional PDCP Duplication TNL List |
|  |  |
| ***Source to WG:*** | Huawei, Deutsche Telekom, Ericsson, Nokia, Nokia Shanghai Bell  |
| ***Source to TSG:*** | R3 |
|  |  |
| ***Work item code:*** | NR\_IIOT-Core |  | ***Date:*** | 2023-08-24 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-16 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | The *Additional PDCP Duplication UP TNL Information* IE was introduced to indicate the additional TNL addresses for the PDCP duplication up to four legs, in the PDU session resource related IEs (see the agreed R3-204503). In the tabular this IE is referring to **UP Transport Parameters** which contains the cell group ID and its associated UP Transport Layer Information.  However, in the ASN.1, it is encoded as UP Transport Layer Information only as follows.  *additional-PDCP-Duplication-UP-TNL-Information UPTransportLayerInformation,*There is no need to refer to the *UP Transport Parameters* IE, because it is understood that there is no need to indicate the cell group ID or to provide more than one TNL address for the *Additional PDCP Duplication UP TNL Information* IE, given the fact that the PDCP duplication is supported with dual connectivity (MCG/SCG). To resolve this issue, it can be considered to update the Tabular to refer to the UP Transport Layer Information.   |
|  |  |
| ***Summary of change:*** | In the Tabular, update the *Additional PDCP Duplication UP TNL Information* IE by referring the UP Transport Layer Information instead of the UP Transport Parameters. Impact Analysis:Impact assessment towards the previous version of the specification (same release): This CR has isolated impact with the previous version of the specification (same release).The impact can be considered isolated because the change only affects the Additional PDCP Duplication UP TNL Information for PDCP duplication. |
|  |  |
| ***Consequences if not approved:*** | The Additional PDCP Duplication UP TNL Information cannot be correctly indicated in the Tabular.  |
|  |  |
| ***Clauses affected:*** | 9.2.1.6, 9.2.1.7, 9.2.1.8, 9.2.1.9, 9.2.1.10, 9.2.1.11, 9.2.1.12, 9.2.1.20, 9.2.1.21, 9.2.1.22 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **x** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **x** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** | Rev0: R3-233960Rev1: R3-234608 Update the cover page based on the online comments. |

|  |
| --- |
| **Change Begins** |

#### 9.2.1.6 PDU Session Resource Setup Response Info – SN terminated

This IE contains the result of the addition of S-NG-RAN node resources related to a PDU session for DRBs configured with an SN terminated bearer option.

| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| --- | --- | --- | --- | --- | --- | --- |
| DL NG-U UP TNL Information at NG-RAN | M |  | UP Transport Layer Information 9.2.3.30 | S-NG-RAN node endpoint of the NG transport bearer. For delivery of DL PDUs. | – |  |
| **DRBs To Be Setup List** |  | *0..1* |  |  | – |  |
| **>DRBs to Be Setup Item** |  | *1 .. <maxnoofDRBs>* |  |  | – |  |
| >>DRB ID | M |  | 9.2.3.33 |  | – |  |
| >>SN UL PDCP UP TNL Information | M |  | UP Transport Parameters 9.2.3. 76 | S-NG-RAN node endpoint(s) of a DRB’s Xn transport bearer at its PDCP resource. For delivery of UL PDUs. | – |  |
| >>DRB QoS | M |  | QoS Flow Level QoS Parameters9.2.3.5 |  | – |  |
| >>PDCP SN Length | O |  | 9.2.3.63 | Indicates the PDCP SN length of the DRB. | – |  |
| >>RLC Mode | M |  | 9.2.3.28 | Indicates the RLC mode to be used in the assisting node. | – |  |
| >>secondary SN UL PDCP UP TNL Information | O |  | UP Transport Parameters 9.2.3.76 | S-NG-RAN node endpoint(s) of a DRB’s Xn transport bearer at its PDCP resource. For delivery of UL PDUs in case of PDCP duplication. | – |  |
| >>Duplication Activation | O |  | 9.2.3.71 | Information on the initial state of UL PDCP duplication.This IE is ignored if the *RLC Duplication Information* IE is present. | – |  |
| >>UL Configuration | O |  | 9.2.3.75 | Information about UL usage in the M-NG-RAN node. This IE is used when the concerned DRB has both MCG resource and SCG resource configured i.e. the concerned DRB is configured as split bearer. | – |  |
| **>>QoS Flows Mapped To DRB List** |  | *1* |  |  | – |  |
| **>>>QoS Flows Mapped To DRB Item** |  | *1 .. <maxnoofQoSFlows>* |  |  | – |  |
| >>>>QoS Flow Identifier | M |  | 9.2.3.10 |  | – |  |
| >>>>MCG requested GBR QoS Flow Information  | O |  | GBR QoS Flow Information9.2.3.6 | This IE contains GBR QoS Flow Information necessary for the MCG part.  | – |  |
| >>>>QoS Flow Mapping Indication | O |  | 9.2.3.79 |  | – |  |
| >>>>Current QoS Parameters Set Index | O |  | Alternative QoS Parameters Set Index9.2.3.103 |  | YES | ignore |
| >>>>Source DL Forwarding IP Address | O |  | Transport Layer Address9.2.3.29 | Identifies the TNL address used by the source node for data forwarding. | YES | ignore |
| **>>Additional PDCP Duplication TNL List** |  | *0..1* |  |  | YES | ignore |
| **>>>Additional PDCP Duplication TNL Item** |  | *1 .. <maxnoofAdditionalPDCPDuplicationTNL>* |  |  | – |  |
| >>>>Additional PDCP Duplication UP TNL Information | M |  | UP Transport Layer Information 9.2.3.30 | S-NG-RAN node endpoint(s) of a DRB’s Xn transport bearer at its PDCP resource. For delivery of UL PDUs in case of additional PDCP duplication. | – |  |
| >>RLC Duplication Information | O |  | 9.2.3.111 | . | – |  |
| Data Forwarding Info from target NG-RAN node | O |  | 9.2.1.16 |  | – |  |
| QoS Flows Not Admitted List | O |  | QoS Flow List with Cause9.2.1.4 |  | – |  |
| Security Result | O |  | 9.2.3.67 |  | – |  |
| DRB IDs taken into use | O |  | DRB List 9.2.1.29 | Indicating the DRB IDs taken into use by the target NG-RAN node, as specified in TS 37.340 [8]. | YES | reject |
| Redundant DL NG-U UP TNL Information at NG-RAN | O |  | UP Transport Layer Information9.2.3.30 | S-NG-RAN node endpoint of the NG transport bearer. For delivery of DL PDUs for the redundant transmission. | YES | ignore |
| Used RSN Information | O |  | Redundant PDU Session Information9.2.3.112 |  | YES | ignore |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofDRBs | Maximum no. of DRBs allowed towards one UE. Value is 32.  |
| maxnoofQoSFlows | Maximum no. of QoS flows. Value is 64 |
| maxnoofAdditionalPDCPDuplicationTNL | Maximum no. of additional PDCP Duplication TNL. Value is 2. |

#### 9.2.1.7 PDU Session Resource Setup Info – MN terminated

This IE contains information for the addition of S-NG-RAN node resources related to a PDU session for DRBs configured with an MN terminated bearer option.

| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| --- | --- | --- | --- | --- | --- | --- |
| PDU Session Type | M |  | 9.2.3.19 |  | – |  |
| **DRBs To Be Setup List** |  | *1* |  |  | – |  |
| **>DRBs to Be Setup Item** |  | *1 .. <maxnoofDRBs>* |  |  | – |  |
| >>DRB ID | M |  | 9.2.3.33 |  | – |  |
| >>MN UL PDCP UP TNL Information | M |  | UP Transport Parameters 9.2.3.76 | M-NG-RAN node endpoint(s) of a DRB’s Xn-U transport bearer at its PDCP resource. For delivery of UL PDUs. | – |  |
| >>RLC Mode | M |  | 9.2.3.28 | Indicates the RLC mode to be used in the assisting node. | – |  |
| >>UL Configuration | O |  | 9.2.3.75 | Information about UL usage in the S-NG-RAN node. This IE is used when the concerned DRB has both MCG resource and SCG resource configured i.e. the concerned DRB is configured as split bearer. | – |  |
| >>DRB QoS | M |  | QoS Flow Level QoS Parameters9.2.3.5 |  | – |  |
| >>PDCP SN Length | O |  | 9.2.3.63 | Indicates the PDCP SN length of the DRB. | – |  |
| >>secondary MN UL PDCP UP TNL Information | O |  | UP Transport Parameters 9.2.3.76 | M-NG-RAN node endpoint(s) of a DRB’s Xn transport bearer at its PDCP resource. For delivery of UL PDUs in case of PDCP duplication. | – |  |
| >>Duplication Activation | O |  | 9.2.3.71 | Information on the initial state of UL PDCP duplication.This IE is ignored if the *RLC Duplication Information* IE is present. | – |  |
| **>>QoS Flows Mapped To DRB List** |  | *1* |  |  | – |  |
| **>>>QoS Flows Mapped To DRB Item** |  | *1 .. <maxnoofQoSFlows>* |  |  | – |  |
| >>>>QoS Flow Identifier  | M |  | 9.2.3.10 |  | – |  |
| >>>>QoS Flow Level QoS Parameters  | M |  | 9.2.3.5 |  | – |  |
| >>>>QoS Flow Mapping Indication | O |  | 9.2.3.79 |  | – |  |
| >>>>TSC Traffic Characteristics | O |  | 9.2.3.114 |  | YES | ignore |
| **>>Additional PDCP Duplication TNL List** |  | *0..1* |  |  | YES | ignore |
| **>>>Additional PDCP Duplication TNL Item** |  | *1 .. <maxnoofAdditionalPDCPDuplicationTNL>* |  |  | – |  |
| >>>>Additional PDCP Duplication UP TNL Information | M |  | UP Transport Layer Information 9.2.3.30 | M-NG-RAN node endpoint(s) of a DRB’s Xn transport bearer at its PDCP resource. For delivery of UL PDUs in case of additional PDCP duplication. | – |  |
| >>RLC Duplication Information | O |  | 9.2.3.111 |  | YES | ignore |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofDRBs | Maximum no. of DRBs allowed towards one UE. Value is 32.  |
| maxnoofQoSFlows | Maximum no. of QoS flows allowed within one PDU session. Value is 64. |
| maxnoofAdditionalPDCPDuplicationTNL | Maximum no. of additional PDCP Duplication TNL. Value is 2. |

#### 9.2.1.8 PDU Session Resource Setup Response Info – MN terminated

This IE contains the result of the addition of S-NG-RAN node resources related to a PDU session for DRBs configured with an MN terminated bearer option.

| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| --- | --- | --- | --- | --- | --- | --- |
| **DRBs Admitted List** |  | *1* |  |  | – |  |
| **>DRBs Admitted Item** |  | *1 .. <maxnoofDRBs>* |  |  | – |  |
| >>DRB ID | M |  | 9.2.3.33 |  | – |  |
| >>SN DL SCG UP TNL Information | M |  | UP Transport Parameters 9.2.3.76 | S-NG-RAN node GTP-U tunnel endpoint(s) of the DRB’s Xn transport at its Lower Layer SCG resource. For delivery of DL PDUs. | – |  |
| >>secondary SN DL SCG UP TNL Information | O |  | UP Transport Parameters 9.2.3.76 | S-NG-RAN node GTP-U tunnel endpoint(s) of the DRB’s Xn transport at its Lower Layer SCG resource. For delivery of DL PDUs in case of PDCP duplication. | – |  |
| >>LCID | O |  | 9.2.3.70 | LCID for primary path or LCID for split secondary path for fallback to split bearer if PDCP duplication is applied | – |  |
| **>>Additional PDCP Duplication TNL List** |  | *0..1* |  |  | YES | ignore |
| **>>>Additional PDCP Duplication TNL Item** |  | *1 .. <maxnoofAdditionalPDCPDuplicationTNL>* |  |  | – |  |
| >>>>Additional PDCP Duplication UP TNL Information | M |  | UP Transport Layer Information 9.2.3.30 | S-NG-RAN node GTP-U tunnel endpoint(s) of the DRB’s Xn transport at its Lower Layer SCG resource. For delivery of DL PDUs in case of additional PDCP duplication. | – |  |
| **>>QoS Flows Mapped To DRB List** |  | *0..1* |  |  | YES | ignore |
| **>>>QoS Flows Mapped To DRB Item** |  | *1 .. <maxnoofQoSFlows>* |  |  | – |  |
| >>>>QoS Flow Identifier  | M |  | 9.2.3.10 |  | – |  |
| >>>>Current QoS Parameters Set Index | M |  | Alternative QoS Parameters Set Index9.2.3.103 |  | – |  |
| **DRBs Not Admitted To Be Setup or Modified List** | O |  | DRB List with Cause9.2.1.28 |  | YES | ignore |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofDRBs | Maximum no. of DRBs allowed towards one UE. Value is 32.  |
| maxnoofAdditionalPDCPDuplicationTNL | Maximum no. of additional PDCP Duplication TNL. Value is 2 |

#### 9.2.1.9 PDU Session Resource Modification Info – SN terminated

This IE contains information related to a PDU session resource for an M-NG-RAN node initiated request to modify DRBs configured with an SN terminated bearer option.

| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| --- | --- | --- | --- | --- | --- | --- |
| UL NG-U UP TNL Information at UPF | O |  | UP Transport Layer Information 9.2.3.30 | UPF endpoint of the NG-U transport bearer. For delivery of UL PDUs | – |  |
| Network Instance | O |  | 9.2.3.85 | This IE shall be ignored if the *Common Network Instance* IE is present. | – |  |
| **QoS Flows To Be Setup List** |  | *0..1* |  |  | – |  |
| **>QoS Flows To Be Setup Item** |  | *1 .. <maxnoofQoSFlows>* |  |  | – |  |
| >>QoS Flow Identifier  | M |  | 9.2.3.10 |  | – |  |
| >>QoS Flow Level QoS Parameters  | M |  | 9.2.3.5 | For GBR QoS flows, this IE contains GBR QoS flow information as received at NG-C  | – |  |
| >>Offered GBR QoS Flow Information  | O |  | GBR QoS Flow Information9.2.3.6 | This IE contains M-Node offered GBR QoS Flow Information.  | – |  |
| >>TSC Traffic Characteristics | O |  | 9.2.3.114 |  | YES | ignore |
| >>Redundant QoS Flow Indicator  | O |  | 9.2.3.118 |  | YES | ignore |
| Data Forwarding and Offloading Info from source NG-RAN node | O |  | 9.2.1.17 | Applicable for the QoS flows contained in the *QoS Flows To Be Setup List* IE. | – |  |
| **QoS Flows To Be Modified List** |  | *0..1* |  |  | – |  |
| **>QoS Flows To Be Modified Item** |  | *1 .. <maxnoofQoSFlows>* |  |  | – |  |
| >>QoS Flow Identifier  | M |  | 9.2.3.10 |  | – |  |
| >>QoS Flow Level QoS Parameters  | O |  | 9.2.3.5 | For GBR QoS flows, this IE contains GBR QoS flow information as received at NG-C  | – |  |
| >>Offered GBR QoS Flow Information  | O |  | GBR QoS Flow Information9.2.3.6 | This IE contains M-Node offered GBR QoS Flow Information.  | – |  |
| >>QoS Flow Mapping Indication | O |  | 9.2.3.79 | This IE is not applicable in this version of the specification. | – |  |
| >>TSC Traffic Characteristics | O |  | 9.2.3.114 |  | YES | ignore |
| >>Redundant QoS Flow Indicator | O |  | 9.2.3.118 |  | YES | ignore |
| QoS Flows To Be Released List |  | *0..1* | QoS Flow List with Cause9.2.1.4 |  | – |  |
| **DRBs To Be Modified List** |  | *0..1* |  |  | – |  |
| **>DRBs to Be Modified Item** |  | *1 .. <maxnoofDRBs>* |  |  | – |  |
| >>DRB ID | M |  | 9.2.3.33 |  | – |  |
| >>MN DL CG UP TNL Information | O |  | UP Transport Parameters 9.2.3.76 | M-NG-RAN node GTP-U endpoint(s) of a DRB’s Xn transport bearer at its lower layer CG resource. For delivery of DL PDUs. | – |  |
| >>secondary MN DL CG UP TNL Information | O |  | UP Transport Parameters 9.2.3.76 | M-NG-RAN node GTP-U endpoint(s) of a DRB’s Xn transport bearer at its lower layer CG resource. For delivery of DL PDUs in case of PDCP duplication. | – |  |
| >>LCID | O |  | 9.2.3.70 | LCID for primary path or LCID for split secondary path for fallback to split bearer if PDCP duplication is applied | – |  |
| >>RLC Status | O |  | 9.2.3.80 |  | – |  |
| **>>Additional PDCP Duplication TNL List** |  | *0..1* |  |  | YES | ignore |
| **>>>Additional PDCP Duplication TNL Item** |  | *1 .. <maxnoofAdditionalPDCPDuplicationTNL>* |  |  | – |  |
| >>>>Additional PDCP Duplication UP TNL Information | M |  | UP Transport Layer Information 9.2.3.30 | M-NG-RAN node GTP-U endpoint(s) of a DRB’s Xn transport bearer at its lower layer CG resource. For delivery of DL PDUs in case of additional PDCP duplication. | – |  |
| DRBs To Be Released List | O |  | DRB List with Cause9.2.1.28 |  | – |  |
| Common Network Instance | O |  | 9.2.3.92 |  | YES | ignore |
| Default DRB Allowed | O |  | 9.2.3.93 |  | YES | ignore |
| Non-GBR Resources Offered | O |  | 9.2.3.98 |  | YES | ignore |
| Redundant UL NG-U UP TNL Information at UPF | O |  | UP Transport Layer Information9.2.3.30 | UPF endpoint of the NG-U transport bearer. For delivery of UL PDUs for the redundant transmission | YES | ignore |
| Redundant Common Network Instance  | O |  | Common Network Instance9.2.3.92 |  | YES | ignore |
| Security Indication | O |  | 9.2.3.52 |  | YES | ignore |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofQoSFlows | Maximum no. of QoS flows. Value is 64. |
| maxnoofAdditionalPDCPDuplicationTNL | Maximum no. of additional PDCP Duplication TNL. Value is 2. |

#### 9.2.1.10 PDU Session Resource Modification Response Info – SN terminated

This IE contains the PDU session resource related result of an M-NG-RAN node initiated request to modify DRBs configured with an SN terminated bearer option.

| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| --- | --- | --- | --- | --- | --- | --- |
| DL NG-U UP TNL Information at NG-RAN | O |  | UP Transport Layer Information 9.2.3.30 | S-NG-RAN node endpoint of the NG transport bearer. For delivery of DL PDUs. | – |  |
| **DRBs To Be Setup List** |  | *0..1* |  |  | – |  |
| **>DRBs to Be Setup Item** |  | *1 .. <maxnoofDRBs>* |  |  | – |  |
| >>DRB ID | M |  | 9.2.3.33 |  | – |  |
| >>SN UL PDCP UP TNL Information | M |  | UP Transport Parameters 9.2.3.76 | S-NG-RAN node endpoint(s) of a DRB’s Xn transport bearer at its PDCP resource. For delivery of UL PDUs. | – |  |
| >>DRB QoS | M |  | QoS Flow Level QoS Parameters9.2.3.5 |  | – |  |
| >>PDCP SN Length | O |  | 9.2.3.63 | Indicates the PDCP SN length of the DRB. | – |  |
| >>RLC Mode | M |  | 9.2.3.28 | Indicates the RLC mode to be used in the assisting node. | – |  |
| >>secondary SN UL PDCP UP TNL Information | O |  | UP Transport Parameters 9.2.3.76 | S-NG-RAN node endpoint(s) of a DRB’s Xn transport bearer at its PDCP resource. For delivery of UL PDUs in case of PDCP duplication. | – |  |
| >>Duplication Activation | O |  | 9.2.3.71 | Information on the initial state of UL PDCP duplication.This IE is ignored if the *RLC Duplication Information* IE is present. | – |  |
| >>UL Configuration | O |  | 9.2.3.75 | Information about UL usage in the S-NG-RAN node. This IE is used when the concerned DRB has both MCG resource and SCG resource configured i.e. the concerned DRB is configured as split bearer. | – |  |
| **>>QoS Flows Mapped To DRB List** |  | *1* |  |  | – |  |
| **>>>QoS Flows Mapped To DRB Item** |  | *1 .. <maxnoofQoSFlows>* |  |  | – |  |
| >>>>QoS Flow Identifier  | M |  | 9.2.3.10 |  | – |  |
| >>>>MCG requested GBR QoS Flow Information  | O |  | GBR QoS Flow Information9.2.3.6 | This IE contains GBR QoS Flow Information necessary for the MCG part.  | – |  |
| >>>>QoS Flow Mapping Indication | O |  | 9.2.3.79 |  | – |  |
| >>>>Current QoS Parameters Set Index | O |  | Alternative QoS Parameters Set Index9.2.3.103 |  | YES | ignore |
| >>>>Source DL Forwarding IP Address | O |  | Transport Layer Address9.2.3.29 | Identifies the TNL address used by the source node for data forwarding. | YES | ignore |
| **>>Additional PDCP Duplication TNL List** |  | *0..1* |  |  | YES | ignore |
| **>>>Additional PDCP Duplication TNL Item** |  | *1 .. <maxnoofAdditionalPDCPDuplicationTNL>* |  |  | – |  |
| >>>>Additional PDCP Duplication UP TNL Information | M |  | UP Transport Layer Information 9.2.3.30 | S-NG-RAN node endpoint(s) of a DRB’s Xn transport bearer at its PDCP resource. For delivery of UL PDUs in case of additional PDCP duplication. | – |  |
| >>RLC Duplication Information | O |  | 9.2.3.111 |  | YES | ignore |
| Data Forwarding Info from target NG-RAN node | O |  | 9.2.1.16 | Applicable for the QoS flows in DRBs to be setup. | – |  |
| **DRBs To Be Modified List** |  | *0..1* |  |  | – |  |
| **>DRBs to Be Modified Item** |  | *1 .. <maxnoofDRBs>* |  |  | – |  |
| >>DRB ID | M |  | 9.2.3.33 |  | – |  |
| >>SN UL PDCP UP TNL Information | O |  | UP Transport Parameters 9.2.3.76 | S-NG-RAN node endpoint(s) of a DRB’s Xn transport bearer at its PDCP resource. For delivery of UL PDUs. | – |  |
| >>DRB QoS | O |  | QoS Flow Level QoS Parameters9.2.3.5 |  | – |  |
| **>>QoS Flows Mapped to DRB List** |  | *0..1* |  | Overwriting the existing QoS Flow List | – |  |
| **>>>QoS Flows Mapped to DRB Item** |  | *1 .. <maxnoofQoSFlows>* |  |  | – |  |
| >>>>QoS Flow Identifier  | M |  | 9.2.3.10 |  | – |  |
| >>>>MCG requested GBR QoS Flow Information  | O |  | GBR QoS Flow Information9.2.3.6 | This IE contains GBR QoS Flow Information necessary for the MCG part.  | – |  |
| >>>>QoS Flow Mapping Indication | O |  | 9.2.3.79 |  | – |  |
| >>>>Current QoS Parameters Set Index | O |  | Alternative QoS Parameters Set Index9.2.3.103 |  | YES | ignore |
| >>>>Source DL Forwarding IP Address | O |  | Transport Layer Address9.2.3.29 | Identifies the TNL address used by the source node for data forwarding. | YES | ignore |
| **>>Additional PDCP Duplication TNL List** |  | *0..1* |  |  | YES | ignore |
| **>>>Additional PDCP Duplication TNL Item** |  | *1 .. <maxnoofAdditionalPDCPDuplicationTNL>* |  |  | – |  |
| >>>>Additional PDCP Duplication UP TNL Information | M |  | UP Transport Layer Information 9.2.3.30 | S-NG-RAN node endpoint(s) of a DRB’s Xn transport bearer at its PDCP resource. For delivery of UL PDUs in case of additional PDCP duplication. | – |  |
| >>RLC Duplication Information | O |  | 9.2.3.111 |  | YES | ignore |
| >>secondary SN UL PDCP UP TNL Information | O |  | UP Transport Parameters 9.2.3.76 | S-NG-RAN node endpoint(s) of a DRB’s Xn transport bearer at its PDCP resource. For delivery of UL PDUs in case of PDCP duplication. | YES | ignore |
| >>PDCP Duplication Configuration | O |  | 9.2.3.86 |  | YES | ignore |
| >>Duplication Activation | O |  | 9.2.3.71 |  | YES | ignore |
| **DRBs To Be Released List** |  | *0..1* |  |  | – |  |
| **>DRBs to Be Released Item** |  | *1 .. <maxnoofDRBs>* |  |  | – |  |
| >>DRB ID | M |  | 9.2.3.33 |  | – |  |
| >>Cause | O |  | 9.2.3.2 |  | – |  |
| Data Forwarding and Offloading Info from source NG-RAN node | O |  | 9.2.1.17 | Contains DL Data Forwarding indications for QoS Flows removed from the SDAP in the SN. | – |  |
| QoS Flows Not Admitted to be Added List | O |  | QoS Flow List with Cause9.2.1.4 |  | – |  |
| QoS Flows Released List | O |  | QoS Flow List with Cause9.2.1.4 |  | – |  |
| DRB IDs taken into use | O |  | DRB List 9.2.1.29 | Indicating the DRB IDs taken into use by the target NG-RAN node, as specified in TS 37.340 [8]. | YES | reject |
| Redundant DL NG-U UP TNL Information at NG-RAN | O |  | UP Transport Layer Information9.2.3.30 | S-NG-RAN node endpoint of the NG transport bearer. For delivery of DL PDUs for the redundant transmission. | YES | ignore |
| Security Result | O |  | 9.2.3.67 |  | YES | ignore |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofDRBs | Maximum no. of DRBs allowed towards one UE. Value is 32.  |
| maxnoofQoSFlows | Maximum no. of QoS flows. Value is 64. |
| maxnoofAdditionalPDCPDuplicationTNL | Maximum no. of additional PDCP Duplication TNL. Value is 2. |

#### 9.2.1.11 PDU Session Resource Modification Info – MN terminated

This IE contains information related to PDU session resource for an M-NG-RAN node initiated request to modify DRBs configured with an MN terminated bearer option.

| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| --- | --- | --- | --- | --- | --- | --- |
| PDU Session Type | M |  | 9.2.3.19 |  | – |  |
| **DRBs To Be Setup List** |  | *0..1* |  |  | – |  |
| **>DRBs to Be Setup Item** |  | *1 .. <maxnoof DRBs>* |  |  | – |  |
| >>DRB ID | M |  | 9.2.3.33 |  | – |  |
| >>MN UL PDCP UP TNL Information | M |  | UP Transport Parameters 9.2.3.76 | M-NG-RAN node endpoint(s) of a DRB’s Xn transport bearer at its PDCP resource. For delivery of UL PDUs. | – |  |
| >>RLC Mode | M |  | 9.2.3.28 | Indicates the RLC mode to be used in the assisting node. | – |  |
| >>UL Configuration | O |  | 9.2.3.75 | Information about UL usage in the S-NG-RAN node. This IE is used when the concerned DRB has both MCG resource and SCG resource configured i.e. the concerned DRB is configured as split bearer. | – |  |
| >>DRB QoS | M |  | QoS Flow Level QoS Parameters9.2.3.5 |  | – |  |
| >>PDCP SN Length | O |  | 9.2.3.63 | Indicates the PDCP SN length of the DRB. | – |  |
| >>secondary MN UL PDCP UP TNL Information | O |  | UP Transport Parameters 9.2.3.76 | M-NG-RAN node endpoint(s) of a DRB’s Xn transport bearer at its PDCP resource. For delivery of UL PDUs in case of PDCP duplication. | – |  |
| >>Duplication Activation | O |  | 9.2.3.71 | Information on the initial state of UL PDCP duplication.This IE is ignored if the *RLC Duplication Information* IE is present. | – |  |
| **>>QoS Flows Mapped to DRB List** |  | *1* |  |  | – |  |
| **>>>QoS Flows Mapped To DRB Item** |  | *1 .. <maxnoofQoSFlows>* |  |  | – |  |
| >>>>QoS Flow Identifier  | M |  | 9.2.3.10 |  | – |  |
| >>>>QoS Flow Level QoS Parameters  | M |  | 9.2.3.5 |  | – |  |
| >>>>QoS Flow Mapping Indication | O |  | 9.2.3.79 |  | – |  |
| **>>Additional PDCP Duplication TNL List** |  | *0..1* |  |  | YES | Ignore |
| **>>>Additional PDCP Duplication TNL Item** |  | *1 .. <maxnoofAdditionalPDCPDuplicationTNL>* |  |  | – |  |
| >>>>Additional PDCP Duplication UP TNL Information | M |  | UP Transport Layer Information 9.2.3.30 | M-NG-RAN node endpoint(s) of a DRB’s Xn transport bearer at its PDCP resource. For delivery of UL PDUs in case of additional PDCP duplication. | – |  |
| >>RLC Duplication Information | O |  | 9.2.3.111 |  | YES | ignore |
| **DRBs To Be Modified List** |  | *0..1* |  |  | – |  |
| **>DRBs to Be Modified Item** |  | *1 .. <maxnoofDRBs>* |  |  | – |  |
| >>DRB ID | M |  | 9.2.3.33 |  | – |  |
| >>MN UL PDCP UP TNL Information | O |  | UP Transport Parameters 9.2.3.76 | M-NG-RAN node endpoint(s) of a DRB’s Xn transport bearer at its PDCP resource. For delivery of UL PDUs. | – |  |
| >>DRB QoS | O |  | QoS Flow Level QoS Parameters9.2.3.5 |  | – |  |
| >>secondary MN UL PDCP UP TNL Information | O |  | UP Transport Parameters 9.2.3.76 | M-NG-RAN node endpoint(s) of a DRB’s Xn transport bearer at its PDCP resource. For delivery of UL PDUs in case of PDCP duplication. | – |  |
| >>UL Configuration | O |  | 9.2.3.75 | Information about UL usage in the S-NG-RAN node. | – |  |
| >>PDCP Duplication Configuration | O |  | 9.2.3.86 |  | – |  |
| >>Duplication Activation | O |  | 9.2.3.71 | Information on the initial state of UL PDCP duplication.This IE is ignored if the *RLC Duplication Information* IE is present. | – |  |
| **>>QoS Flows Mapped To DRB List** |  | *0..1* |  | Overwriting the existing QoS Flow List | – |  |
| **>>>QoS Flows Mapped To DRB Item** |  | *1 .. <maxnoof QoS Flows>* |  |  | – |  |
| >>>>QoS Flow Identifier  | M |  | 9.2.3.10 |  | – |  |
| >>>>QoS Flow Level QoS Parameters  | M |  | 9.2.3.5 |  | – |  |
| >>>>QoS Flow Mapping Indication | O |  | 9.2.3.79 |  | – |  |
| **>>Additional PDCP Duplication TNL List** |  | *0..1* |  |  | YES | ignore |
| **>>>Additional PDCP Duplication TNL Item** |  | *1 .. <maxnoofAdditionalPDCPDuplicationTNL>* |  |  | – |  |
| >>>>Additional PDCP Duplication UP TNL Information | M |  | UP Transport Layer Information 9.2.3.30 | M-NG-RAN node endpoint(s) of a DRB’s Xn transport bearer at its PDCP resource. For delivery of UL PDUs in case of additional PDCP duplication. | – |  |
| >>RLC Duplication Information | O |  | 9.2.3.111 |  | YES | ignore |
| DRBs To Be Released List | O |  | DRB List with Cause9.2.1.28 |  | – |  |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofDRBs | Maximum no. of DRBs allowed towards one UE. Value is 32.  |
| maxnoofQoSFlows | Maximum no. of QoS flows allowed within one PDU session. Value is 64. |
| maxnoofAdditionalPDCPDuplicationTNL | Maximum no. of additional PDCP Duplication TNL. Value is 2. |

#### 9.2.1.12 PDU Session Resource Modification Response Info – MN terminated

This IE contains the PDU session resource related result of an M-NG-RAN node initiated modification of DRBs configured with an MN terminated bearer option.

| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| --- | --- | --- | --- | --- | --- | --- |
| **DRBs Admitted to be Setup or Modified List** |  | *1* |  |  | – |  |
| **>DRBs Admitted to be Setup or Modified Item** |  | *1 .. <maxnoofDRBs>* |  |  | – |  |
| >>DRB ID | M |  | 9.2.3.33 |  | – |  |
| >>SN DL SCG UP TNL Information | O |  | UP Transport Parameters 9.2.3.76 | S-NG-RAN node GTP-U tunnel endpoint(s) of the DRB’s Xn transport at its Lower Layer SCG resource. For delivery of DL PDUs. | – |  |
| >>secondary SN DL SCG UP TNL Information | O |  | UP Transport Parameters 9.2.3.76 | S-NG-RAN node GTP-U tunnel endpoint(s) of the DRB’s Xn transport at its Lower Layer SCG resource. For delivery of DL PDUs in case of PDCP duplication. | – |  |
| >>LCID | O |  | 9.2.3.70 | LCID for primary path or LCID for split secondary path for fallback to split bearer if PDCP duplication is applied | – |  |
| **>>Additional PDCP Duplication TNL List** |  | *0..1* |  |  | YES | ignore |
| **>>>Additional PDCP Duplication TNL Item** |  | *1 .. <maxnoofAdditionalPDCPDuplicationTNL>* |  |  | – |  |
| >>>>Additional PDCP Duplication UP TNL Information | M |  | UP Transport Layer Information 9.2.3.30 | S-NG-RAN node GTP-U tunnel endpoint(s) of the DRB’s Xn transport at its Lower Layer SCG resource. For delivery of DL PDUs in case of additional PDCP duplication. | – |  |
| **>>QoS Flows Mapped To DRB List** |  | *0..1* |  |  | YES | ignore |
| **>>>QoS Flows Mapped To DRB Item** |  | *1 .. <maxnoofQoSFlows>* |  |  | – |  |
| >>>>QoS Flow Identifier  | M |  | 9.2.3.10 |  | – |  |
| >>>>Current QoS Parameters Set Index | O |  | Alternative QoS Parameters Set Index9.2.3.103 |  | – |  |
| DRBs Released List | O |  | DRB List9.2.1.29 |  | – |  |
| DRBs Not Admitted To Be Setup or Modified List | O |  | DRB List with Cause9.2.1.28 |  | – |  |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofDRBs | Maximum no. of DRBs allowed towards one UE. Value is 32.  |
| maxnoofAdditionalPDCPDuplicationTNL | Maximum no. of additional PDCP Duplication TNL. Value is 2. |

<<<<<<<<<<<<<<<<<<<< Unmodified Text Omitted >>>>>>>>>>>>>>>>>>>>

#### 9.2.1.20 PDU Session Resource Modification Required Info – SN terminated

This IE contains PDU session resource information of an S-NG-RAN node initiated modification request of DRBs configured with an SN terminated bearer option.

| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| --- | --- | --- | --- | --- | --- | --- |
| DL NG-U UP TNL Information at NG-RAN | O |  | UP Transport Layer Information 9.2.3.30 | S-NG-RAN node endpoint of the NG-U transport bearer. For delivery of DL PDUs. | – |  |
| QoS Flows To Be Released List | O |  | QoS Flow List with Cause9.2.1.4 |  | – |  |
| Data Forwarding and Offloading Info from source NG-RAN node | O |  | 9.2.1.17 | This IE only applies to QoS flows included in the *QoS FlowS To Be Released List* IE. | – |  |
| **DRBs To Be Setup List** |  | *0..1* |  |  | – |  |
| **>DRBs to Be Setup Item** |  | *1 .. <maxnoofDRBs>* |  |  | – |  |
| >>DRB ID | M |  | 9.2.3.33 |  | – |  |
| >>PDCP SN Length | O |  | 9.2.3.63 | Indicates the PDCP SN length of the DRB. | – |  |
| >>SN UL PDCP UP TNL Information | M |  | UP Transport Parameters 9.2.3.76 | S-NG-RAN node endpoint(s) of a DRB’s Xn transport bearer at its PDCP resource. For delivery of UL PDUs. | – |  |
| >>DRB QoS | M |  | QoS Flow Level QoS Parameters9.2.3.5 |  | – |  |
| >>secondary SN UL PDCP UP TNL Information | O |  | UP Transport Parameters 9.2.3.76 | S-NG-RAN node endpoint(s) of a DRB’s Xn transport bearer at its PDCP resource. For delivery of UL PDUs in case of PDCP Duplication. | – |  |
| >>Duplication Activation | O |  | 9.2.3.71 | Information on the initial state of UL PDCP duplication.This IE is ignored if the *RLC Duplication Information* IE is present. | – |  |
| >>UL Configuration | O |  | 9.2.3.75 | Information about UL usage in the S-NG-RAN node. This IE is used when the concerned DRB has both MCG resource and SCG resource configured i.e. the concerned DRB is configured as split bearer. | – |  |
| **>>QoS Flows Mapped To DRB List** |  | *1* |  |  | – |  |
| **>>>QoS Flows Mapped To DRB Item** |  | *1 .. <maxnoofQoSFlows>* |  |  | – |  |
| >>>>QoS Flow Identifier | M |  | 9.2.3.10 |  | – |  |
| >>>>MCG requested GBR QoS Flow Information  | O |  | GBR QoS Flow Information9.2.3.6 | This IE contains GBR QoS Flow Information necessary for the MCG part.  | – |  |
| >>>>QoS Flow Mapping Indication | O |  | 9.2.3.79 |  | – |  |
| >>RLC Mode | M |  | 9.2.3.28 | Indicates the RLC mode at the assisting node. | – |  |
| **>>Additional PDCP Duplication TNL List** |  | *0..1* |  |  | YES | ignore |
| **>>>Additional PDCP Duplication TNL Item** |  | *1 .. <maxnoofAdditionalPDCPDuplicationTNL>* |  |  | – |  |
| >>>>Additional PDCP Duplication UP TNL Information | M |  | UP Transport Layer Information 9.2.3.30 | S-NG-RAN node endpoint(s) of a DRB’s Xn transport bearer at its PDCP resource. For delivery of UL PDUs in case of additional PDCP Duplication. | – |  |
| >>RLC Duplication Information | O |  | 9.2.3.111 |  | YES | ignore |
| **DRBs To Be Modified List** |  | *0..1* |  |  | – |  |
| **>DRBs to Be Modified Item** |  | *1 .. <maxnoofDRBs>* |  |  | – |  |
| >>DRB ID | M |  | 9.2.3.33 |  | – |  |
| >>SN UL PDCP UP TNL Information | O |  | UP Transport Parameters 9.2.3.76 | S-NG-RAN node endpoint(s) of a DRB’s Xn transport bearer at its PDCP resource. For delivery of UL PDUs. | – |  |
| >>DRB QoS | O |  | QoS Flow Level QoS Parameters9.2.3.5 |  | – |  |
| >>secondary SN UL PDCP UP TNL Information | O |  | UP Transport Parameters 9.2.3.76 | S-NG-RAN node endpoint(s) of a DRB’s Xn transport bearer at its PDCP resource. For delivery of UL PDUs in case of PDCP Duplication. | – |  |
| >>UL Configuration | O |  | 9.2.3.75 | Information about UL usage in the S-NG-RAN node. | – |  |
| >>PDCP Duplication Configuration | O |  | 9.2.3.86 |  | – |  |
| >>Duplication Activation | O |  | 9.2.3.71 | This IE is ignored if the *RLC Duplication Information* IE is present. | – |  |
| **>>QoS Flows Mapped to DRB List** |  | *0..1* |  | Overwriting the existing QoS Flow List | – |  |
| **>>>QoS Flows Mapped to DRB Item** |  | *1 .. <maxnoofQoSFlows>* |  |  | – |  |
| >>>>QoS Flow Identifier | M |  | 9.2.3.10 |  | – |  |
| >>>>MCG requested GBR QoS Flow Information  | O |  | GBR QoS Flow Information9.2.3.6 | This IE contains GBR QoS Flow Information necessary for the MCG part.  | – |  |
| >>>>QoS Flow Mapping Indication | O |  | 9.2.3.79 |  | – |  |
| **>>Additional PDCP Duplication TNL List** |  | *0..1* |  |  | YES | ignore |
| **>>>Additional PDCP Duplication TNL Item** |  | *1 .. <maxnoofAdditionalPDCPDuplicationTNL>* |  |  | – |  |
| >>>>Additional PDCP Duplication UP TNL Information | M |  | UP Transport Layer Information 9.2.3.30 | S-NG-RAN node endpoint(s) of a DRB’s Xn transport bearer at its PDCP resource. For delivery of UL PDUs in case of additional PDCP Duplication. | – |  |
| >>RLC Duplication Information | O |  | 9.2.3.111 |  | YES | ignore |
| **DRBs To Be Released List** | O |  | DRB List with Cause9.2.1.28 |  | – |  |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofDRBs | Maximum no. of DRBs allowed towards one UE. Value is 32. |
| maxnoofQoSFlows | Maximum no. of QoS flows. Value is 64. |
| maxnoofAdditionalPDCPDuplicationTNL | Maximum no. of additional PDCP Duplication TNL. Value is 2. |

#### 9.2.1.21 PDU Session Resource Modification Confirm Info – SN terminated

This IE contains the PDU session resource related result of an S-NG-RAN node initiated modification of DRBs configured with an SN terminated bearer option.

| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| --- | --- | --- | --- | --- | --- | --- |
| UL NG-U UP TNL Information at UPF | O |  | UP Transport Layer Information 9.2.3.30 | UPF endpoint of the NG-U transport bearer. For delivery of UL PDUs | – |  |
| **DRBs Admitted to be Setup or Modified List** |  | *1* |  |  | – |  |
| **>DRBs Admitted to be Setup or Modified Item** |  | *1 .. <maxnoofDRBs>* |  |  | – |  |
| >>DRB ID | M |  | 9.2.3.33 |  | – |  |
| >>MN DL CG UP TNL Information | O |  | UP Transport Parameters 9.2.3.76 | M-NG-RAN node endpoint(s) of the DRB’s Xn transport at its Lower Layer CG resource. For delivery of DL PDUs. | – |  |
| >>secondary MN DL CG UP TNL Information | O |  | UP Transport Parameters 9.2.3.76 | M-NG-RAN node endpoint(s) of the DRB’s Xn transport at its Lower Layer CG resource. For delivery of DL PDUs at the case of PDCP duplication. | – |  |
| >>LCID | O |  | 9.2.3.70 |  Shall be ignored by the S-NG-RAN node if received. | – |  |
| **>>Additional PDCP Duplication TNL List** |  | *0..1* |  |  | YES | ignore |
| **>>>Additional PDCP Duplication TNL Item** |  | *1 .. <maxnoofAdditionalPDCPDuplicationTNL>* |  |  | – |  |
| >>>>Additional PDCP Duplication UP TNL Information | M |  | UP Transport Layer Information 9.2.3.30 | M-NG-RAN node endpoint(s) of the DRB’s Xn transport at its Lower Layer CG resource. For delivery of DL PDUs at the case of additional PDCP duplication. | – |  |
| DRBs Not Admitted To Be Setup or Modified List | O |  | DRB List with Cause9.2.1.28 |  | – |  |
| Data Forwarding Info from target NG-RAN node | O |  | 9.2.1.16 | Forwarding Addresses for both, QoS flow and DRB level offloading. | – |  |
| DRB IDs taken into use | O |  | DRB List 9.2.1.29 | Indicating the DRB IDs taken into use by the target NG-RAN node, as specified in TS 37.340 [8]. | YES | reject |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofDRBs | Maximum no. of DRBs allowed towards one UE. Value is 32. |
| maxnoofQoSFlows | Maximum no. of QoS flows. Value is 64. |
| maxnoofAdditionalPDCPDuplicationTNL | Maximum no. of additional PDCP Duplication TNL. Value is 2. |

#### 9.2.1.22 PDU Session Resource Modification Required Info – MN terminated

This IE contains PDU session resource information of an S-NG-RAN node initiated modification request of DRBs configured with an MN terminated bearer option.

| IE/Group Name | Presence | Range | IE type and reference | Semantics description | Criticality | Assigned Criticality |
| --- | --- | --- | --- | --- | --- | --- |
| **DRBs To Be Modified List** | O |  |  |  | – |  |
| **>DRBs To Be Modified Item** |  | *1..<maxnoofDRBs>* |  |  | – |  |
| >>DRB ID | M |  | 9.2.3.33 |  | – |  |
| >>SN DL SCG UP TNL Information | M |  | UP Transport Layer Information 9.2.3.30 | S-NG-RAN node endpoint of a DRB’s Xn transport bearer. For delivery of DL PDUs. | – |  |
| >>secondary SN DL SCG UP TNL Information | O |  | UP Transport Layer Information 9.2.3.30 | S-NG-RAN node endpoint of a DRB’s Xn transport bearer. For delivery of DL PDUs in case of PDCP Duplication | – |  |
| >>LCID | O |  | 9.2.3.70 | LCID for primary path or LCID for split secondary path for fallback to split bearer if PDCP duplication is applied | – |  |
| >>RLC Status | O |  | 9.2.3.80 |  | – |  |
| **>>Additional PDCP Duplication TNL List** |  | *0..1* |  |  | YES | ignore |
| **>>>Additional PDCP Duplication TNL Item** |  | *1 .. <maxnoofAdditionalPDCPDuplicationTNL>* |  |  | – |  |
| >>>>Additional PDCP Duplication UP TNL Information | M |  | UP Transport Layer Information 9.2.3.30 | S-NG-RAN node endpoint of a DRB’s Xn transport bearer. For delivery of DL PDUs in case of additional PDCP Duplication | – |  |
| DRBs To Be Released List | O |  | DRB List with Cause9.2.1.28 |  | – |  |

|  |  |
| --- | --- |
| Range bound | Explanation |
| maxnoofDRBs | Maximum no. of DRBs. Value is 32. |
| maxnoofAdditionalPDCPDuplicationTNL | Maximum no. of additional PDCP Duplication TNL. Value is 2. |

<<<<<<<<<<<<<<<<<<<< Unmodified Text Omitted >>>>>>>>>>>>>>>>>>>>

### 9.3.5 Information Element definitions

-- ASN1START

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

--

-- Information Element Definitions

--

-- \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

**<For Information Only>**

Additional-PDCP-Duplication-TNL-List ::= SEQUENCE (SIZE(1..maxnoofAdditionalPDCPDuplicationTNL)) OF Additional-PDCP-Duplication-TNL-Item

Additional-PDCP-Duplication-TNL-Item ::= SEQUENCE {
 additional-PDCP-Duplication-UP-TNL-Information UPTransportLayerInformation,
 iE-Extensions ProtocolExtensionContainer { { Additional-PDCP-Duplication-TNL-ExtIEs} } OPTIONAL,
 ...
}

Additional-PDCP-Duplication-TNL-ExtIEs XNAP-PROTOCOL-EXTENSION ::= {
 ...
}

|  |
| --- |
| **Change Ends** |