**3GPP TSG-RAN WG3 Meeting #121 R3-234069**

**Toulouse, France, 21 – 25 Aug, 2023**

**Title:** (TP for SON BLCR for TS 38.420): Introduction of RACH Indication

**Source:** Huawei, China Telecom, CMCC

**Agenda item:** 10.2.3

**Document Type:** other

# 1. Introduction

This document contains a TP to SON BLCR for TS 38.420 for RACH optimisation .

# Annex: TP to TS 38.420 BL CR

*Start of the changes*

### 6.2.9 Data exchange for self-optimisation procedures

The data exchange for self-optimisation procedures are used to transfer failure and mobility related information among NG-RAN nodes to enable self-optimisation

- Failure Indication

- Handover report

- Mobility Settings Change

- Access and Mobility Indication

- SCG Failure Information Report

- SCG Failure Transfer

The following procedures are used to transfer SON related information among NG-RAN nodes to enable self-optimisation.

- RACH Indication

*End of changes*