**3GPP TSG-RAN WG3 Meeting #123 *R3-241064***

**Athens, GR, 26 Feb – 01 Mar, 2023**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  | **38.300** | **CR** | **<CR#>** | **rev** | **-** | **Current version:** | **18.0.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **x** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Correction on MRO |
|  |  |
| ***Source to WG:*** | Huawei, Deutsche Telekom, Nokia, Nokia Shanghai Bell |
| ***Source to TSG:*** | R3 |
|  |  |
| ***Work item code:*** | NR\_ENDC\_SON\_MDT\_enh2-Core |  | ***Date:*** | 2024-02-29 |
|  |  |  |  |  |
| ***Category:*** | F |  | ***Release:*** | Rel-18 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | Existing text is missing a reference to the more detailed behaviour in 37.340The section header does not include addition. |
|  |  |
| ***Summary of change:*** | Simplified the text and added reference to 37.340Modified the section header. |
|  |  |
| ***Consequences if not approved:*** | No reference to the detailed behaviour. |
|  |  |
| ***Clauses affected:*** | 15.5.2.6 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **x** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **x** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **x** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

15.5.2.6 PSCell addition/change failure

For analysis of PSCell addition/change failures, the UE makes the SCG Failure Information available to the MN. If the MN can perform an initial analysis, it transfers the SCG Failure Information together with the analysis results to the relevant SN as defined in TS 37.340 [21].