**3GPP TSG- Meeting #**

**, Japan, - 2024**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.3* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  |  | **CR** |  | **rev** | **-** | **Current version:** |  |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **X** | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** |  | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | , Ericsson, CMCC | | | | | | | | | |
| ***Source to TSG:*** |  | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** |  | | | | |  | ***Date:*** | | |  |
|  |  | | | |  | |  | | |  |
| ***Category:*** |  |  | | | | | ***Release:*** | | |  |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)  Rel-20 (Release 20)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | RAN3 agreed on the following in RAN3#121-bis meeting:  “Both of the following two options are adopted to support PTM configuration provision during RRC Release procedure in split gNB scenario:  Option 1: CU retrieves the PTM configuration from DU via CU initiated Multicast context setup/modification procedure.  Option 2: During active MBS multicast sessions, the DU always ensures that the CU is provided with the latest PTM configuration via a new DU initiated Multicast context modification procedure.”  It is expected to capture above RAN3 understanding in stage 2 spec. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | RAN3 understanding on F1AP interactions for multicast reception in RRC\_INACTIVE, in section 7.7.3.  Impact Analysis:  Impact assessment towards the previous version of the specification (same release):  This CR has an isolated impact towards the previous version of the specification (same release). | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | The interaction on F1AP is not clearly defined for the newly introduced multicast reception for UE in RRC\_INACTIVE state. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 7.7.3 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

// change starts.

7.7.3 Support of Multicast reception for UEs in RRC\_INACTIVE

F1AP supports:

* enabling and disabling multicast reception for UEs in RRC\_INACTIVE state for a specific multicast MBS session on cell level.
* retrieval of PTM configuration information from the the gNB-DU by means of the gNB-CU triggered Multicast Context Modification procedure.
* keeping the gNB-CU updated during active multicast MBS sessions with the latest PTM configuration by means of the gNB-DU initiated Multicast Context Notification procedure.

The gNB-CU decides whether multicast reception in RRC\_INACTIVE state is applied.

// change ends.