{"text_format":"1","workbook":"xlsx","n_sheets":4,"sheets":["Cover","Parameters","FR1 CP 1T2R","FR2 CP 1T2R"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Cover","index":0,"n_rows":8,"n_cols":10,"rows_kept":8,"cut":false,"hidden":false,"merged":[]}
[]
[null,"3GPP TSG-RAN WG4 Meeting #95-e",null,null,null,null,null,null,null,"R4-2006250"]
[null,"Electronic meeting,  25 May - 5 June, 2020"]
[]
[null,"Source: CATT"]
[null,"Title: Summary of ideal and impairment results for NR PUSCH with 30% throughput test point"]
[null,"Agenda: 6.18.2.1"]
[null,"Document for: Information"]

{"sheet":"Parameters","index":1,"n_rows":12,"n_cols":5,"rows_kept":12,"cut":false,"hidden":false,"merged":[[1,2,1,4],[7,2,7,4],[6,2,6,4]]}
[]
[null,null,"Parameters for deriving performance requirements"]
[null,null,"Ideal Span Threshold",2,"dB"]
[null,null,"Impairment Span Threshold",4,"dB"]
[]
[]
[null,"Notes","1. Call function DerivingPerfReq()"]
[null,null,"2. If the ruls does not apply, or fails, -100dB or less will be returned"]
[null,null,null,-100,"Not enough input"]
[null,null,null,-101,"Input should be pairs"]
[null,null,null,-102,"Too large span for impairment"]
[null,null,null,-103,"After removal iteration, not enough input"]

{"sheet":"FR1 CP 1T2R","index":2,"n_rows":6,"n_cols":29,"rows_kept":6,"cut":false,"hidden":false,"merged":[[0,27,0,28],[0,13,0,14],[0,15,0,16],[0,17,0,18],[0,23,0,24],[0,11,0,12],[0,6,1,6],[0,19,0,20],[0,21,0,22],[0,25,0,26],[0,0,1,0],[0,1,1,1],[0,3,1,3],[0,8,1,8],[0,9,0,10],[0,7,1,7],[0,2,1,2],[0,4,1,4],[0,5,1,5]]}
[" waveform","Tx/Rx","PUSCH mapping type","SCS and BW","MCS level","Propagation condition","DMRS","38.104 req","38.141 req","Samsung",null,"ZTE",null,"CMCC",null,"CATT",null,"Nokia",null,"Huawei",null,"Ericsson",null,"China Telecom",null,"SPAN",null,"AVERAGE"]
[null,null,null,null,null,null,null,null,null,"Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment"]
["CP-OFDM","1T2R","type A","15kHz, 5MHz","MCS16","TDLC300-100","DMRS 1+1",{"$f":"DerivingPerfReq(J3:Y3)","v":2.9},{"$f":"IF(H3>-100,H3+0.6,H3)","v":3.5},0.87,2.87,null,null,null,null,0.53,3.0300000000000002,0.59,3.09,0.53,2.5299999999999998,0.6,2.93,0.68,2.68,{"$f":"MAX(J3,L3,N3,P3,R3,T3,V3,X3)-MIN(J3,L3,N3,P3,R3,T3,V3,X3)","v":0.33999999999999997},{"$f":"MAX(K3,M3,O3,Q3,S3,U3,W3,Y3)-MIN(K3,M3,O3,Q3,S3,U3,W3,Y3)","v":0.56000000000000005},{"$f":"AVERAGE(J3,L3,N3,P3,R3,T3,V3,X3)","v":0.6333333333333333},2.855]
["CP-OFDM","1T2R","type A","30kHz, 10MHz","MCS16","TDLC300-100","DMRS 1+1",{"$f":"DerivingPerfReq(J4:Y4)","v":2.8},{"$f":"IF(H4>-100,H4+0.6,H4)","v":3.4},0.93,2.93,null,null,null,null,0.44,2.94,0.63,3.13,0.53,2.5299999999999998,0.5,2.5099999999999998,0.95,2.95,{"$f":"MAX(J4,L4,N4,P4,R4,T4,V4,X4)-MIN(J4,L4,N4,P4,R4,T4,V4,X4)","v":0.51},0.62000000000000011,0.66333333333333344,2.8316666666666666]
["CP-OFDM","1T2R"," type B","15kHz, 5MHz","MCS16","TDLC300-100","DMRS 1+1",{"$f":"DerivingPerfReq(J5:Y5)","v":2.8},3.4,0.85,2.85,null,null,null,null,0.49,2.99,0.61,3.11,0.74,2.74,0.6,2.64,0.7,2.7,0.36,0.46999999999999975,0.66499999999999992,2.8383333333333334]
["CP-OFDM","1T2R","type B","30kHz, 10MHz","MCS16","TDLC300-100","DMRS 1+1",{"$f":"DerivingPerfReq(J6:Y6)","v":2.9},3.5,0.92,2.92,null,null,null,null,0.37,2.87,0.62,3.12,0.56999999999999995,2.57,0.5,2.91,0.9,2.9,0.55000000000000004,0.55000000000000027,0.64666666666666661,2.8816666666666664]

{"sheet":"FR2 CP 1T2R","index":3,"n_rows":10,"n_cols":30,"rows_kept":10,"cut":false,"hidden":false,"merged":[[0,0,1,0],[0,1,1,1],[0,2,1,2],[0,3,1,3],[0,4,1,4],[0,5,1,5],[0,6,1,6],[0,7,1,7],[0,28,0,29],[0,14,0,15],[0,16,0,17],[0,18,0,19],[0,20,0,21],[0,22,0,23],[0,26,0,27],[0,8,1,8],[0,9,1,9],[0,10,0,11],[0,24,0,25],[0,12,0,13]]}
["waveform","Tx/Rx","PUSCH mapping type","SCS and BW","MCS level","Propagation condition","DMRS","PTRS","38.104 req","38.141 req","Samsung",null,"ZTE",null,"CMCC",null,"CATT",null,"Nokia",null,"Huawei",null,"Ericsson",null,"China Telecom",null,"SPAN",null,"AVERAGE"]
[null,null,null,null,null,null,null,null,null,null,"Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment"]
["CP-OFDM","1T2R","type B","60kHz, 50MHz","MCS16","TDLA30-300","DMRS 1","K_PTRS=2,\nL_PTRS=1",{"$f":"DerivingPerfReq(K3:Z3)","v":4},{"$f":"IF(I3>-100,I3+0.6,I3)","v":4.5999999999999996},1.57,4.07,null,null,null,null,1.28,3.7800000000000002,0.92,4.0200000000000005,1.69,4.1900000000000004,0.9,4.18,null,null,{"$f":"MAX(K3,M3,O3,Q3,S3,U3,W3,Y3)-MIN(K3,M3,O3,Q3,S3,U3,W3,Y3)","v":0.78999999999999992},{"$f":"MAX(L3,N3,P3,R3,T3,V3,X3,Z3)-MIN(L3,N3,P3,R3,T3,V3,X3,Z3)","v":0.41000000000000014},{"$f":"AVERAGE(K3,M3,O3,Q3,S3,U3,W3,Y3)","v":1.272},{"$f":"AVERAGE(L3,N3,P3,R3,T3,V3,X3,Z3)","v":4.048}]
["CP-OFDM","1T2R","type B","60kHz, 50MHz","MCS16","TDLA30-300","DMRS 1","No",{"$f":"DerivingPerfReq(K4:Z4)","v":3.5},{"$f":"IF(I4>-100,I4+0.6,I4)","v":4.0999999999999996},1.27,3.77,null,null,null,null,0.98,3.48,0.57999999999999996,3.68,1.1000000000000001,3.6,0.65,3.93,0.69,2.69,{"$f":"MAX(K4,M4,O4,Q4,S4,U4,W4,Y4)-MIN(K4,M4,O4,Q4,S4,U4,W4,Y4)","v":0.69000000000000006},{"$f":"MAX(L4,N4,P4,R4,T4,V4,X4,Z4)-MIN(L4,N4,P4,R4,T4,V4,X4,Z4)","v":1.2400000000000002},{"$f":"AVERAGE(K4,M4,O4,Q4,S4,U4,W4,Y4)","v":0.8783333333333333},{"$f":"AVERAGE(L4,N4,P4,R4,T4,V4,X4,Z4)","v":3.5250000000000004}]
["CP-OFDM","1T2R","type B","120kHz, 50MHz","MCS16","TDLA30-300","DMRS 1","K_PTRS=2,\nL_PTRS=1",{"$f":"DerivingPerfReq(K5:Z5)","v":4},4.5999999999999996,1.73,4.2300000000000004,null,null,null,null,1.46,3.96,1.1399999999999999,4.24,1.78,4.28,1.05,3.5,null,null,0.73,0.78000000000000025,1.4319999999999999,4.0419999999999998]
["CP-OFDM","1T2R","type B","120kHz, 50MHz","MCS16","TDLA30-300","DMRS 1","No",3.6,4.2,1.3,3.8,null,null,null,null,1.1599999999999999,3.66,0.62,3.72,1.25,3.75,0.8,3.52,1.02,3.02,0.68,0.7799999999999998,1.0250000000000001,3.5783333333333331]
["CP-OFDM","1T2R","type B","60kHz, 50MHz","MCS16","TDLA30-300","DMRS 1+1","K_PTRS=2,\nL_PTRS=1",3.7,4.3,1.32,3.82,null,null,null,null,0.85000000000000009,3.35,0.81,3.91,1.03,3.53,0.5,3.69,null,null,0.82000000000000006,0.56000000000000005,0.90199999999999991,3.66]
["CP-OFDM","1T2R","type B","60kHz, 50MHz","MCS16","TDLA30-300","DMRS 1+1","No",3.1,3.7,0.97,3.47,null,null,null,null,0.45,2.95,0.46,3.56,0.71,3.21,0.25,3.03,0.45,2.4500000000000002,0.72,1.1099999999999999,0.54833333333333334,3.1116666666666668]
["CP-OFDM","1T2R","type B","120kHz, 50MHz","MCS16","TDLA30-300","DMRS 1+1","K_PTRS=2,\nL_PTRS=1",3.7,4.3,1.38,3.88,null,null,null,null,0.90999999999999992,3.41,0.96,4.0600000000000005,1.34,3.84,0.55000000000000004,3.37,null,null,0.82999999999999985,0.69000000000000039,1.028,3.7120000000000006]
["CP-OFDM","1T2R","type B","120kHz, 50MHz","MCS16","TDLA30-300","DMRS 1+1","No",3.2,3.8000000000000003,0.98,3.48,null,null,null,null,0.41,2.91,0.47,3.5700000000000003,0.97,3.47,0.3,2.99,0.8,2.8,0.67999999999999994,0.77000000000000046,0.65499999999999992,3.2033333333333336]