Naming convention:

psc_{codec}_b{Bearer starting number}_{Bearer ending number}_s{Sequence number}.rtp

codec = h263 / h264
Bearer starting number = 1 / 6
Bearer ending number = 5 / 10
(note: bearer 1, 2, … , 5 are 64 kbps; bearer 6, 7, … , 10 are 128 kbps. Hence a file named psc_h26*_b6_10_s*.rtp is the encoded file to be transmitted by any of the bearers 6, 7, …, 10)
Sequence = 1 = stunt, 2 = bar, 3 = party

