**3GPP TSG-SA5 Meeting #132e *S5-204223***

**e-meeting 17th 28th August 2020** Revision of S5-20xxxx

|  |
| --- |
| *CR-Form-v11.4* |
| **CHANGE REQUEST** |
|  |
|  | **32.291** | **CR** | **0261** | **rev** | **1** | **Current version:** | **16.4.2** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Add the NSPA charging attribute for convergedcharging service |
|  |  |
| ***Source to WG:*** | Huawei |
| ***Source to TSG:*** | S5 |
|  |  |
| ***Work item code:*** | 5GS\_NSPACH |  | ***Date:*** | 2020-08-25 |
|  |  |  |  |  |
| ***Category:*** | **B** |  | ***Release:*** | Rel-16 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)**Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)* |
|  |  |
| ***Reason for change:*** | As per the TS 28.201, the network slice performance and analytics charging is introduced.The corresponding attributes and open API for NS performance and analytics charging for convergedcharging service should be added. |
|  |  |
| ***Summary of change:*** | Add the attributes and open API for NS performance and analytics charging for convergedcharging service. |
|  |  |
| ***Consequences if not approved:*** | The NS performance and analytics charging stage 3 for convergedcharging service is incomplete.  |
|  |  |
| ***Clauses affected:*** | 2, 6.1.6.1,6.1.6.2.x(New),6.1.6.3.4,7.x(New),A.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | Implement the 6.1.6.2.x after 6.1.6.2.5.Implement the 7.x after 7.5. |

|  |
| --- |
| **First change** |

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TS 32.240: "Telecommunication management; Charging management; Charging architecture and principles".

[2] - [13] Void.

[14] 3GPP TS 32.254: "Telecommunication management; Charging management; Exposure function Northbound Application Program Interfaces (APIs) charging ".

[15] - [28] Void.

[29] 3GPP TS 32.274: "Telecommunication management; Charging management;Short Message Service (SMS) charging".

[30] 3GPP TS 32.255: "Telecommunication management; Charging management; 5G Data connectivity domain charging; stage 2".

[31] 3GPP TS 32.256: "Telecommunication management; Charging management; 5G connection and mobility domain charging; stage 2".

[32] - [49] Void.

[50] - [57] Void.

[58] 3GPP TS 32.290: "Telecommunication management; Charging management; 5G system; Services, operations and procedures of charging using Service Based Interface (SBI).

[59] - [99] Void.

[100] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

[101] 3GPP TR 21.900: "Technical Specification Group working methods".

[102] - [199] Void

[200] - [203] Void

[204] - [255] Void

[256] 3GPP TS 28.554: "Management and orchestration;5G end to end Key Performance Indicators (KPI)".

[257] - [298] Void

[299] 3GPP TS 29.500: "5G System; Technical Realization of Service Based Architecture; Stage 3".

[300] 3GPP TS 29.501: "5G System; Principles and Guidelines for Services Definition; Stage 3".

[301] 3GPP TS 29.594: "5G System; Spending Limit Control Service; Stage 3".

[302] 3GPP TS 29.512: "5G System; Session Management Policy Control Service; Stage 3".

[303] 3GPP TS 24.501: "Non-Access-Stratum (NAS) Protocol for 5G System (5GS); Stage 3".

[304] 3GPP TS 38.413: "NG-RAN; NG Application Protocol (NGAP)".

[305] 3GPP TS 29.520: "5G System; Network Data Analytics Services;Stage 3".

[306] - [370] Void

[371] 3GPP TS 29.571: "5G System; Common Data Types for Service Based Interfaces; Stage 3".

[372] - [389] Void

[390] 3GPP TS 33.501: "Security architecture and procedures for 5G System".

[391] - [399] Void

[400] Void.

[401] IETF RFC 7540: "Hypertext Transfer Protocol Version 2 (HTTP/2) ".

[402] IETF RFC 8259: "The JavaScript Object Notation (JSON) Data Interchange Format ".

[403] - [499] Void.

[500] OpenAPI: "OpenAPI 3.0.0 Specification", <https://github.com/OAI/OpenAPI-Specification/blob/master/versions/3.0.0.md>.

[501] - [599] Void.

|  |
| --- |
| **Next change** |

#### 6.1.6.1 General

This subclause specifies the application data model supported by the API.

The Nchf\_ConvergedCharging Service API allows the NF consumer to consume the converged charging service from the CHF as defined in 3GPP TS 32.290 [58].

Table 6.1.6.1-1 specifies the data types defined for the ConvergedCharging service based interface protocol.

Table 6.1.6.1-1: Nchf\_ ConvergedCharging specific Data Types

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | Section defined | Description | Applicability |
| ChargingDataRequest | 6.1.6.2.1.16.1.6.2.2.1 | Describes the attributes of Charging Data Request to CHF for initial, update and termination of the charging session. |  |
| ChargingDataResponse | 6.1.6.2.1.26.1.6.2.2.2 | Describes the attributes of Charging Data Response from CHF on charging session initial, update and termination. |  |
| ChargingNotifyRequest | 6.1.6.2.1.3 | Describes Notifications about events that occurred in request message. |  |
| ChargingNotifyResponse | 6.1.6.2.1.16 | Describes the response of notification. |  |

Table 6.1.6.1-2 specifies data types re-used by the Nchf\_ConvergedCharging service based interface protocol from other specifications, including a reference to their respective specifications and when needed, a short description of their use within the Nchf\_ConvergedCharging service based interface.

Table 6.1.6.1-2: Nchf\_ConvergedCharging re-used Data Types

|  |  |  |  |
| --- | --- | --- | --- |
| Data type | Reference | Comments | Applicability |
| Supi | 3GPP TS 29.571 [371] | The identification of the user (i.e. IMSI, NAI, GLI, GCI).(NOTE 1) |  |
| Uint32 | 3GPP TS 29.571 [371] | Unsigned 32-bit integers |  |
| Uint64 | 3GPP TS 29.571 [371] | Unsigned 64-bit integers |  |
| PduSessionId | 3GPP TS 29.571 [371] | The identification of the PDU session. |  |
| PduSessionType | 3GPP TS 29.571 [371] | the type of a PDU session |  |
| Uri | 3GPP TS 29.571 [371] | String providing an URI |  |
| AccessType | 3GPP TS 29.571 [371] | The identification of the type of access network. |  |
| DateTime | 3GPP TS 29.571 [371] | The time. |  |
| ChargingId | 3GPP TS 29.571 [371] | Charging identifier allowing correlation of charging information |  |
| RatType | 3GPP TS 29.571 [371] | The identification of the RAT type. |  |
| RatingGroup | 3GPP TS 29.571 [371] | The identification of the rating group |  |
| Ipv4Addr | 3GPP TS 29.571 [371] | Ipv4 address.  |  |
| Ipv6Prefix | 3GPP TS 29.571 [371] | The Ipv6 prefix allocated for the user. |  |
| Ipv6Addr | 3GPP TS 29.571 [371] | Ipv6 Address. |  |
| Pei | 3GPP TS 29.571 [371] | The Identification of a Permanent Equipment. |  |
| TimeZone | 3GPP TS 29.571 [371] | Time zone information |  |
| NfInstanceId | 3GPP TS 29.571 [371] | String uniquely identifying a NF instance. |  |
| Gpsi | 3GPP TS 29.571 [371] | String identifying a Gpsi |  |
| DefaultQosInformation | 3GPP TS 29.571 [371] | Identifies the information of the default QoS. |  |
| SubscribedDefaultQos | 3GPP TS 29.571 [371] | subscribed default QoS. |  |
| AuthorizedDefaultQos | 3GPP TS 29.512 [302] | Authorized default QoS. |  |
| Ambr | 3GPP TS 29.571 [371] | Aggregate Maximum Bit rate  |  |
| QosData | 3GPP TS 29.512 [302] | Contains QoS parameters |  |
| UserLocation | 3GPP TS 29.571 [371] | User location information |  |
| PlmnId | 3GPP TS 29.571 [371] | PLMN id |  |
| Guami | 3GPP TS 29.571 [371] | Globally Unique AMF Identifier |  |
| DurationSec | 3GPP TS 29.571 [371] | Identifies a period of time in units of seconds. |  |
| Snssai | 3GPP TS 29.571 [371] | SNSSAI |  |
| ProblemDetails | 3GPP TS 29.571 [371] | additional details of the error |  |
| ServiceId | 3GPP TS 29.571 [371] | Identifier of service |  |
| SscMode | 3GPP TS 29.571 [371] | SSC Mode type |  |
| PresenceInfo | 3GPP TS 29.571 [371] | PRA information including PRAId, PRA element list and PRA status |  |
| Qfi | 3GPP TS 29.571 [371] | QoS flow identifier designated as "Qfi". |  |
| AmfId | 3GPP TS 29.571 [371] | AMF identifier |  |
| Dnn | 3GPP TS 29.571 [371] | Data Network Name |  |
| GroupId | 3GPP TS 29.571 [371] | Identifies a group |  |
| Bytes | 3GPP TS 29.571 [371] | String with format "byte" |  |
| Tai | 3GPP TS 29.571 [371] | Tracking Area Identifier |  |
| Area | 3GPP TS 29.571 [371] | List of TACs or Operator specific codes |  |
| CoreNetworkType | 3GPP TS 29.571 [371] | 5GC or EPC |  |
| ServiceAreaRestriction | 3GPP TS 29.571 [371] | Service Area restriction |  |
| GlobalRanNodeId | 3GPP TS 29.571 [371] | Global RAN Node Id |  |
| QosCharacteristics | 3GPP TS 29.512 [302] | Map of QoS characteristics for non standard 5QIs and non-preconfigured 5QIs. |  |
| SupportedFeatures | 3GPP TS 29.571 [371] | See 3GPP TS 29.500 [4] clause 6.6 |  |
| NsiLoadLevelInfo | 3GPP TS 29.520 [305] | Represents the load level information for an S-NSSAI and the associated network slice instance |  |
| ServiceExperienceInfo | 3GPP TS 29.520 [305] | ServiceExperience |  |
| Throughput | 3GPP TS 28.541 [255] | Throughput |  |
| NOTE 1: A SUPI containing GLI or GCI is used to support 5G-RG and FN-RG in scenarios of wireline network. |

|  |
| --- |
| **Next change** |

##### 6.1.6.2.x NS performance and analytics Specified Data Type

###### 6.1.6.2.X.1 Type ChargingDataRequest

This clause is additional attributes of the type ChargingDataRequest defined in clause 6.1.6.2.x.1 for NS performance and analytics charging described in 3GPP TS 28.201[201].

Table 6.1.6.2.x.1-1: NS performance and analytics Specified attribute of type ChargingDataRequest

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| tenantIdentifier | string | OM  | 0..1 | This field contains the identification of the subscriber of the network slice |  |
| nSPAChargingInformation | NSPAChargingInformation | OC | 0..1 | This field holds the network slice information, which is reported to the CHF |  |

###### 6.1.6.2.X.2 Type ChargingDataResponse

This clause is additional attributes of the type ChargingDataResponse defined in clause 6.1.6.2.x.2 for NS performance and analytics charging described in 3GPP TS 28.201[201].

Table 6.1.6.2.x.2-1: NS performance and analytics Specified attribute of type ChargingDataResponse

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
|  |  |  |  |  |  |

###### 6.1.6.2.x.3 Type UsedUnitContainer

This clause is additional portion of the type UsedUnitContainer defined in clause 6.1.6.2.1.10 for NS performance and analytics charging described in 3GPP TS 28.201[201].

Table 6.1.6.2.x.3-1: NS performance and analytics charging of type UsedUnitContainer

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| nSPAChargingInformation | NSPAContainerInformation | OC | 0..1 | the network slice performance and analytics container specific information. |  |

###### 6.1.6.2.X.4 Type NSPAChargingInformation

Table 6.1.6.2.X.4-1: Definition of type NSPAChargingInformation

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| singleNSSAI | Snssai | M | 0..1 | This field holds single Network Slice Selection Assistance Information for performance reporting. |  |

###### 6.1.6.2.X.5 Type NSPAContainerInformation

Table 6.1.6.2.X.5-1: Definition of type NSPAContainerInformation

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Attribute name | Data type | P | Cardinality | Description | Applicability |
| latency | integer | OC | 0..1 | This field holds latency  |  |
| throughput | Throughput | OC | 0..1 | This field holds throughput. |  |
| maximumUtilizedBandwidth | string | OC | 0..1 | This field holds maximum utilized bandwidth. |  |
| maximumPacketLossRate | string | OC | 0..1 | This field holds maximum packet loss rate. |  |
| serviceExperienceStatisticsData | ServiceExperienceInfo | OC | 0..1 | This field holds service experience statistics data. |  |
| theNumberOfPDUSessions | integer | OC | 0..1 | This field holds the number of PDU sessions. |  |
| theNumberOfRegisteredSubscribers | integer | OC | 0..1 | This field holds the number of registered subscribers. |  |
| loadLevel | NsiLoadLevelInfo | OC | 0..1 | This field holds the load level of network slice. |  |

|  |
| --- |
| **Next change** |

##### 6.1.6.3.4 Enumeration: NodeFunctionality

Table 6.1.6.3.4-1: Enumeration NodeFunctionality

|  |  |  |
| --- | --- | --- |
| Enumeration value | Description | Applicability |
| SMF | This field identifies that NF is a SMF. |  |
| AMF | This field identifies that NF is a AMF. |  |
| SMSF | This field identifies that NF service consumer is a SMSF. |  |
| SGW | This field identifies that node is an SGW, only applicable for interworking with EPC. |  |
| I\_SMF | This field identifies that node is an I-SMF, only applicable for PDU session served by SMF + I-SMF. |  |
| CEF | This field identifies that NF is a CEF. |  |

|  |
| --- |
| **Next change** |

## 7.X Bindings for NS performance and Analytics charging

Table 7.X-1: Bindings of CDR field, Information Element and Resource Attribute for NS performance and Analytics charging

| Information Element | CDR Field | Resource Attribute |
| --- | --- | --- |
|  |  | **ChargingDataRequest** |
| Tenant Identifier | Tenant Identifier | /tenantIdentifier |
| Multiple Unit Usage | List of Multiple Unit Usage | /multipleUnitUsage |
| Used Unit Container | Used Unit Container  | /multipleUnitUsage/usedUnitContainer |
| NSPA Container Information | NSPA Container Information | /multipleUnitUsage/usedUnitContainer/nSPAContanierInformation |
| Latency | Latency | /multipleUnitUsage/usedUnitContainer/nSPAContanierInformation/latency |
| Throughput | Throughput | /multipleUnitUsage/usedUnitContainer/nSPAContanierInformation/throughput |
| Maximum utilized bandwidth | Maximum utilized bandwidth | /multipleUnitUsage/usedUnitContainer/nSPAContanierInformation/maximumUtilizedBandwidth |
| Maximum packet loss rate | Maximum packet loss rate | /multipleUnitUsage/usedUnitContainer/nSPAContanierInformation/maximumPacketLossRate |
| Service Experience statistics data | Service Experience statistics data | /multipleUnitUsage/usedUnitContainer/nSPAContanierInformation/serviceExperienceStatisticsData |
| The number of PDU sessions | The number of PDU sessions | /multipleUnitUsage/usedUnitContainer/nSPAContanierInformation/theNumberOfPDUSessions |
| The number of Registered Subscribers | The number of Registered Subscribers | /multipleUnitUsage/usedUnitContainer/nSPAContanierInformation/theNumberOfRegisteredSubscribers |
| Load level | Load level | /multipleUnitUsage/usedUnitContainer/nSPAContanierInformation/loadLevel |
| NSPA Charging Information | NSPA Charging Information | /nSPAChargingInformation |
| Single NSSAI | Single NSSAI | /nSPAChargingInformation/singleNSSAI |
|  |  | **ChargingDataResponse** |
| - | - | - |

|  |
| --- |
| **Next change** |

## A.2 Nchf\_ConvergedCharging API

openapi: 3.0.0

info:

 title: Nchf\_ConvergedCharging

 version: 3.0.0.alpha-4

 description: |

 ConvergedCharging Service © 2019, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).

 All rights reserved.

externalDocs:

 description: >

 3GPP TS 32.291 V16.4.0: Telecommunication management; Charging management;

 5G system, charging service; Stage 3.

 url: 'http://www.3gpp.org/ftp/Specs/archive/32\_series/32.291/'

servers:

 - url: '{apiRoot}/nchf-convergedcharging/v3'

 variables:

 apiRoot:

 default: https://example.com

 description: apiRoot as defined in subclause 4.4 of 3GPP TS 29.501.

paths:

 /chargingdata:

 post:

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/ChargingDataRequest'

 responses:

 '201':

 description: Created

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/ChargingDataResponse'

 '400':

 description: Bad request

 content:

 application/problem+json:

 schema:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

 '403':

 description: Forbidden

 content:

 application/problem+json:

 schema:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

 '404':

 description: Not Found

 content:

 application/problem+json:

 schema:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '410':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/410'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 callbacks:

 chargingNotification:

 '{$request.body#/notifyUri}':

 post:

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/ChargingNotifyRequest'

 responses:

 '204':

 description: 'No Content, Notification was succesfull'

 '400':

 description: Bad request

 content:

 application/problem+json:

 schema:

 $ref: >-

 TS29571\_CommonData.yaml#/components/schemas/ProblemDetails

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 '/chargingdata/{ChargingDataRef}/update':

 post:

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/ChargingDataRequest'

 parameters:

 - name: ChargingDataRef

 in: path

 description: a unique identifier for a charging data resource in a PLMN

 required: true

 schema:

 type: string

 responses:

 '200':

 description: OK. Updated Charging Data resource is returned

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/ChargingDataResponse'

 '400':

 description: Bad request

 content:

 application/problem+json:

 schema:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

 '403':

 description: Forbidden

 content:

 application/problem+json:

 schema:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

 '404':

 description: Not Found

 content:

 application/problem+json:

 schema:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '410':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/410'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

 '/chargingdata/{ChargingDataRef}/release':

 post:

 requestBody:

 required: true

 content:

 application/json:

 schema:

 $ref: '#/components/schemas/ChargingDataRequest'

 parameters:

 - name: ChargingDataRef

 in: path

 description: a unique identifier for a charging data resource in a PLMN

 required: true

 schema:

 type: string

 responses:

 '204':

 description: No Content.

 '404':

 description: Not Found

 content:

 application/problem+json:

 schema:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

 '401':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/401'

 '410':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/410'

 '411':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/411'

 '413':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/413'

 '500':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/500'

 '503':

 $ref: 'TS29571\_CommonData.yaml#/components/responses/503'

 default:

 $ref: 'TS29571\_CommonData.yaml#/components/responses/default'

components:

 schemas:

 ChargingDataRequest:

 type: object

 properties:

 subscriberIdentifier:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 tenantIdentifier:

 type: string nfConsumerIdentification:

 $ref: '#/components/schemas/NFIdentification'

 invocationTimeStamp:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 invocationSequenceNumber:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 retransmissionIndicator:

 type: boolean

 oneTimeEvent:

 type: boolean

 oneTimeEventType:

 $ref: '#/components/schemas/oneTimeEventType'

 notifyUri:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 supportedFeatures:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

 serviceSpecificationInfo:

 type: string

 multipleUnitUsage:

 type: array

 items:

 $ref: '#/components/schemas/MultipleUnitUsage'

 minItems: 0

 triggers:

 type: array

 items:

 $ref: '#/components/schemas/Trigger'

 minItems: 0

 pDUSessionChargingInformation:

 $ref: '#/components/schemas/PDUSessionChargingInformation'

 roamingQBCInformation:

 $ref: '#/components/schemas/RoamingQBCInformation'

 sMSChargingInformation:

 $ref: '#/components/schemas/SMSChargingInformation'

 nEFChargingInformation:

 $ref: '#/components/schemas/NEFChargingInformation'

 registrationChargingInformation:

 $ref: '#/components/schemas/RegistrationChargingInformation'

 n2ConnectionChargingInformation:

 $ref: '#/components/schemas/N2ConnectionChargingInformation'

 locationReportingChargingInformation:

 $ref: '#/components/schemas/LocationReportingChargingInformation'

 nSPAChargingInformation:

 $ref: '#/components/schemas/NSPAChargingInformation'

 required:

 - nfConsumerIdentification

 - invocationTimeStamp

 - invocationSequenceNumber

 ChargingDataResponse:

 type: object

 properties:

 invocationTimeStamp:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 invocationSequenceNumber:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 invocationResult:

 $ref: '#/components/schemas/InvocationResult'

 sessionFailover:

 $ref: '#/components/schemas/SessionFailover'

 supportedFeatures:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SupportedFeatures'

 multipleUnitInformation:

 type: array

 items:

 $ref: '#/components/schemas/MultipleUnitInformation'

 minItems: 0

 triggers:

 type: array

 items:

 $ref: '#/components/schemas/Trigger'

 minItems: 0

 pDUSessionChargingInformation:

 $ref: '#/components/schemas/PDUSessionChargingInformation'

 roamingQBCInformation:

 $ref: '#/components/schemas/RoamingQBCInformation'

 required:

 - invocationTimeStamp

 - invocationSequenceNumber

 ChargingNotifyRequest:

 type: object

 properties:

 notificationType:

 $ref: '#/components/schemas/NotificationType'

 reauthorizationDetails:

 type: array

 items:

 $ref: '#/components/schemas/ReauthorizationDetails'

 minItems: 0

 required:

 - notificationType

 ChargingNotifyResponse:

 type: object

 properties:

 invocationResult:

 $ref: '#/components/schemas/InvocationResult'

 NFIdentification:

 type: object

 properties:

 nFName:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

 nFIPv4Address:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

 nFIPv6Address:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Addr'

 nFPLMNID:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnId'

 nodeFunctionality:

 $ref: '#/components/schemas/NodeFunctionality'

 nFFqdn:

 type: string

 required:

 - nodeFunctionality

 MultipleUnitUsage:

 type: object

 properties:

 ratingGroup:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RatingGroup'

 requestedUnit:

 $ref: '#/components/schemas/RequestedUnit'

 usedUnitContainer:

 type: array

 items:

 $ref: '#/components/schemas/UsedUnitContainer'

 minItems: 0

 uPFID:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

 required:

 - ratingGroup

 InvocationResult:

 type: object

 properties:

 error:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ProblemDetails'

 failureHandling:

 $ref: '#/components/schemas/FailureHandling'

 Trigger:

 type: object

 properties:

 triggerType:

 $ref: '#/components/schemas/TriggerType'

 triggerCategory:

 $ref: '#/components/schemas/TriggerCategory'

 timeLimit:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

 volumeLimit:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 volumeLimit64:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 maxNumberOfccc:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 required:

 - triggerType

 - triggerCategory

 MultipleUnitInformation:

 type: object

 properties:

 resultCode:

 $ref: '#/components/schemas/ResultCode'

 ratingGroup:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RatingGroup'

 grantedUnit:

 $ref: '#/components/schemas/GrantedUnit'

 triggers:

 type: array

 items:

 $ref: '#/components/schemas/Trigger'

 minItems: 0

 validityTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

 quotaHoldingTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'

 finalUnitIndication:

 $ref: '#/components/schemas/FinalUnitIndication'

 timeQuotaThreshold:

 type: integer

 volumeQuotaThreshold:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 unitQuotaThreshold:

 type: integer

 uPFID:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

 required:

 - ratingGroup

 RequestedUnit:

 type: object

 properties:

 time:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 totalVolume:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 uplinkVolume:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 downlinkVolume:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 serviceSpecificUnits:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 UsedUnitContainer:

 type: object

 properties:

 serviceId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ServiceId'

 quotaManagementIndicator:

 $ref: '#/components/schemas/QuotaManagementIndicator'

 triggers:

 type: array

 items:

 $ref: '#/components/schemas/Trigger'

 minItems: 0

 triggerTimestamp:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 time:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 totalVolume:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 uplinkVolume:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 downlinkVolume:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 serviceSpecificUnits:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 eventTimeStamps:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 localSequenceNumber:

 type: integer

 pDUContainerInformation:

 $ref: '#/components/schemas/PDUContainerInformation'

 nSPAContainerInformation:

 $ref: '#/components/schemas/NSPAContainerInformation'

 required:

 - localSequenceNumber

 GrantedUnit:

 type: object

 properties:

 tariffTimeChange:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 time:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 totalVolume:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 uplinkVolume:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 downlinkVolume:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 serviceSpecificUnits:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 FinalUnitIndication:

 type: object

 properties:

 finalUnitAction:

 $ref: '#/components/schemas/FinalUnitAction'

 restrictionFilterRule:

 $ref: '#/components/schemas/IPFilterRule'

 filterId:

 type: string

 redirectServer:

 $ref: '#/components/schemas/RedirectServer'

 required:

 - finalUnitAction

 RedirectServer:

 type: object

 properties:

 redirectAddressType:

 $ref: '#/components/schemas/RedirectAddressType'

 redirectServerAddress:

 type: string

 required:

 - redirectAddressType

 - redirectServerAddress

 ReauthorizationDetails:

 type: object

 properties:

 serviceId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ServiceId'

 ratingGroup:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RatingGroup'

 quotaManagementIndicator:

 $ref: '#/components/schemas/QuotaManagementIndicator'

 PDUSessionChargingInformation:

 type: object

 properties:

 chargingId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ChargingId'

 homeProvidedChargingId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ChargingId'

 userInformation:

 $ref: '#/components/schemas/UserInformation'

 userLocationinfo:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

 presenceReportingAreaInformation:

 type: object

 additionalProperties:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PresenceInfo'

 minProperties: 0

 uetimeZone:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

 pduSessionInformation:

 $ref: '#/components/schemas/PDUSessionInformation'

 unitCountInactivityTimer:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DurationSec'
 rANSecondaryRATUsageReport:

 $ref: '#/components/schemas/RANSecondaryRATUsageReport'

 UserInformation:

 type: object

 properties:

 servedGPSI:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

 servedPEI:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Pei'

 unauthenticatedFlag:

 type: boolean

 roamerInOut:

 $ref: '#/components/schemas/RoamerInOut'

 PDUSessionInformation:

 type: object

 properties:

 networkSlicingInfo:

 $ref: '#/components/schemas/NetworkSlicingInfo'

 pduSessionID:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PduSessionId'

 pduType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PduSessionType'

 sscMode:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SscMode'

 hPlmnId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnId'

 servingNetworkFunctionID:

 $ref: '#/components/schemas/ServingNetworkFunctionID'

 ratType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

 dnnId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Dnn'

 dnnSelectionMode:

 $ref: '#/components/schemas/dnnSelectionMode'

 chargingCharacteristics:

 type: string

 chargingCharacteristicsSelectionMode:

 $ref: '#/components/schemas/ChargingCharacteristicsSelectionMode'

 startTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 stopTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 3gppPSDataOffStatus:

 $ref: '#/components/schemas/3GPPPSDataOffStatus'

 sessionStopIndicator:

 type: boolean

 pduAddress:

 $ref: '#/components/schemas/PDUAddress'

 diagnostics:

 $ref: '#/components/schemas/Diagnostics'

 authorizedQoSInformation:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/AuthorizedDefaultQos'

 subscribedQoSInformation:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/SubscribedDefaultQos'

 authorizedSessionAMBR:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ambr'

 subscribedSessionAMBR:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ambr'

 servingCNPlmnId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PlmnId'

 required:

 - pduSessionID

 - dnnId

 PDUContainerInformation:

 type: object

 properties:

 timeofFirstUsage:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 timeofLastUsage:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 qoSInformation:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/QosData'

 qoSCharacteristics:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/QosCharacteristics'

 afChargingIdentifier:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ChargingId'

 userLocationInformation:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

 uetimeZone:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

 rATType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

 servingNodeID:

 type: array

 items:

 $ref: '#/components/schemas/ServingNetworkFunctionID'

 minItems: 0

 presenceReportingAreaInformation:

 type: object

 additionalProperties:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PresenceInfo'

 minProperties: 0

 3gppPSDataOffStatus:

 $ref: '#/components/schemas/3GPPPSDataOffStatus'

 sponsorIdentity:

 type: string

 applicationserviceProviderIdentity:

 type: string

 chargingRuleBaseName:

 type: string

 NSPAContainerInformation:

 type: object

 properties:

 latency:

 type: integer

 throughput:

 type: Throughput

 maximumUtilizedBandwidth:

 type: string

 maximumPacketLossRate:

 type: string

 serviceExperienceStatisticsData:

 type: ServiceExperienceInfo

 theNumberOfPDUSessions:

 type: integer

 theNumberOfRegisteredSubscribers:

 type: integer

 loadLevel:

 type: NsiLoadLevelInfo

 NSPAChargingInformation:

 type: object

 properties:

 singleNSSAI:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 required:

 - sNSSAI

 NetworkSlicingInfo:

 type: object

 properties:

 sNSSAI:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 required:

 - sNSSAI

 PDUAddress:

 type: object

 properties:

 pduIPv4Address:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv4Addr'

 pduIPv6AddresswithPrefix:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Ipv6Addr'

 pduAddressprefixlength:

 type: integer

 iPv4dynamicAddressFlag:

 type: boolean

 iPv6dynamicPrefixFlag:

 type: boolean

 ServingNetworkFunctionID:

 type: object

 properties:

 servingNetworkFunctionInformation:

 $ref: '#/components/schemas/NFIdentification'

 aMFId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/AmfId'

 required:

 - servingNetworkFunctionInformation

 RoamingQBCInformation:

 type: object

 properties:

 multipleQFIcontainer:

 type: array

 items:

 $ref: '#/components/schemas/MultipleQFIcontainer'

 minItems: 0

 uPFID:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/NfInstanceId'

 roamingChargingProfile:

 $ref: '#/components/schemas/RoamingChargingProfile'

 MultipleQFIcontainer:

 type: object

 properties:

 triggers:

 type: array

 items:

 $ref: '#/components/schemas/Trigger'

 minItems: 0

 triggerTimestamp:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 time:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 totalVolume:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 uplinkVolume:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 downlinkVolume:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 localSequenceNumber:

 type: integer

 qFIContainerInformation:

 $ref: '#/components/schemas/QFIContainerInformation'

 required:

 - localSequenceNumber

 QFIContainerInformation:

 type: object

 properties:

 qFI:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Qfi'

 reportTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 timeofFirstUsage:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 timeofLastUsage:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 qoSInformation:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/QosData'

 qoSCharacteristics:

 $ref: 'TS29512\_Npcf\_SMPolicyControl.yaml#/components/schemas/QosCharacteristics'

 userLocationInformation:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

 uetimeZone:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

 presenceReportingAreaInformation:

 type: object

 additionalProperties:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PresenceInfo'

 minProperties: 0

 rATType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

 servingNetworkFunctionID:

 type: array

 items:

 $ref: '#/components/schemas/ServingNetworkFunctionID'

 minItems: 0

 3gppPSDataOffStatus:

 $ref: '#/components/schemas/3GPPPSDataOffStatus'

 3gppChargingId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ChargingId'

 diagnostics:

 $ref: '#/components/schemas/Diagnostics'

 enhancedDiagnostics:

 type: array

 items:

 type: string

 required:

 - reportTime

 RoamingChargingProfile:

 type: object

 properties:

 triggers:

 type: array

 items:

 $ref: '#/components/schemas/Trigger'

 minItems: 0

 partialRecordMethod:

 $ref: '#/components/schemas/PartialRecordMethod'

 SMSChargingInformation:

 type: object

 properties:

 originatorInfo:

 $ref: '#/components/schemas/OriginatorInfo'

 recipientInfo:

 type: array

 items:

 $ref: '#/components/schemas/RecipientInfo'

 minItems: 0

 userEquipmentInfo:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Pei'

 userLocationinfo:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

 uetimeZone:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

 rATType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

 sMSCAddress:

 type: string

 sMDataCodingScheme:

 type: integer

 sMMessageType:

 $ref: '#/components/schemas/SMMessageType'

 sMReplyPathRequested:

 $ref: '#/components/schemas/ReplyPathRequested'

 sMUserDataHeader:

 type: string

 sMStatus:

 type: string

 sMDischargeTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 numberofMessagesSent:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 sMServiceType:

 $ref: '#/components/schemas/SMServiceType'

 sMSequenceNumber:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 sMSresult:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 submissionTime:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 sMPriority:

 $ref: '#/components/schemas/SMPriority'

 messageReference:

 type: string

 messageSize:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 messageClass:

 $ref: '#/components/schemas/MessageClass'

 deliveryReportRequested:

 $ref: '#/components/schemas/DeliveryReportRequested'

 OriginatorInfo:

 type: object

 properties:

 originatorSUPI:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 originatorGPSI:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

 originatorOtherAddress:

 $ref: '#/components/schemas/SMAddressInfo'

 originatorReceivedAddress:

 $ref: '#/components/schemas/SMAddressInfo'

 originatorSCCPAddress:

 type: string

 sMOriginatorInterface:

 $ref: '#/components/schemas/SMInterface'

 sMOriginatorProtocolId:

 type: string

 RecipientInfo:

 type: object

 properties:

 recipientSUPI:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Supi'

 recipientGPSI:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Gpsi'

 recipientOtherAddress:

 $ref: '#/components/schemas/SMAddressInfo'

 recipientReceivedAddress:

 $ref: '#/components/schemas/SMAddressInfo'

 recipientSCCPAddress:

 type: string

 sMDestinationInterface:

 $ref: '#/components/schemas/SMInterface'

 sMrecipientProtocolId:

 type: string

 SMAddressInfo:

 type: object

 properties:

 sMaddressType:

 $ref: '#/components/schemas/SMAddressType'

 sMaddressData:

 type: string

 sMaddressDomain:

 $ref: '#/components/schemas/SMAddressDomain'

 RecipientAddress:

 type: object

 properties:

 recipientAddressInfo:

 $ref: '#/components/schemas/SMAddressInfo'

 sMaddresseeType:

 $ref: '#/components/schemas/SMAddresseeType'

 MessageClass:

 type: object

 properties:

 classIdentifier:

 $ref: '#/components/schemas/ClassIdentifier'

 tokenText:

 type: string

 SMAddressDomain:

 type: object

 properties:

 domainName:

 type: string

 3GPPIMSIMCCMNC:

 type: string

 SMInterface:

 type: object

 properties:

 interfaceId:

 type: string

 interfaceText:

 type: string

 interfacePort:

 type: string

 interfaceType:

 $ref: '#/components/schemas/InterfaceType'

 RANSecondaryRATUsageReport:

 type: object

 properties:

 rANSecondaryRATType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

 qosFlowsUsageReports:

 type: array

 items:

 $ref: '#/components/schemas/QosFlowsUsageReport'

 Diagnostics:

 type: integer

 IPFilterRule:

 type: string

 QosFlowsUsageReport:

 type: object

 properties:

 qFI:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Qfi'

 startTimestamp:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 endTimestamp:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/DateTime'

 uplinkVolume:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 downlinkVolume:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint64'

 NEFChargingInformation:

 type: object

 properties:

 groupIdentifier:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/GroupId'

 aPIDirection:

 $ref: '#/components/schemas/APIDirection'

 aPITargetNetworkFunction:

 $ref: '#/components/schemas/NFIdentification'

 aPIResultCode:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uint32'

 aPIName:

 type: string

 aPIReference:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Uri'

 aPIContent:

 type: string

 required:

 - aPIName

 RegistrationChargingInformation:

 type: object

 properties:

 registrationMessagetype:

 $ref: '#/components/schemas/RegistrationMessageType'

 userInformation:

 $ref: '#/components/schemas/UserInformation'

 userLocationinfo:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

 uetimeZone:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

 rATType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

 5GMMCapability:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Bytes'

 mICOModeIndication:

 $ref: '#/components/schemas/MICOModeIndication'

 smsIndication:

 $ref: '#/components/schemas/SmsIndication'

 taiList:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Tai'

 minItems: 0

 serviceAreaRestriction:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ServiceAreaRestriction'

 minItems: 0

 requestedNSSAI:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 minItems: 0

 allowedNSSAI:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 minItems: 0

 rejectedNSSAI:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 minItems: 0

 required:

 - registrationMessagetype

 N2ConnectionChargingInformation:

 type: object

 properties:

 n2ConnectionMessageType:

 $ref: '#/components/schemas/N2ConnectionMessageType'

 userInformation:

 $ref: '#/components/schemas/UserInformation'

 userLocationinfo:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

 uetimeZone:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

 rATType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

 amfUeNgapId:

 type: integer

 ranUeNgapId:

 type: integer

 ranNodeId:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/GlobalRanNodeId'

 restrictedRatList:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

 minItems: 0

 forbiddenAreaList:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Area'

 minItems: 0

 serviceAreaRestriction:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/ServiceAreaRestriction'

 minItems: 0

 restrictedCnList:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/CoreNetworkType'

 minItems: 0

 allowedNSSAI:

 type: array

 items:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/Snssai'

 minItems: 0

 rrcEstCause:

 type: string

 pattern: '^[0-9a-fA-F]+$'

 required:

 - n2ConnectionMessageType

 LocationReportingChargingInformation:

 type: object

 properties:

 locationReportingMessageType:

 $ref: '#/components/schemas/LocationReportingMessageType'

 userInformation:

 $ref: '#/components/schemas/UserInformation'

 userLocationinfo:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/UserLocation'

 uetimeZone:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/TimeZone'

 rATType:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/RatType'

 presenceReportingAreaInformation:

 type: object

 additionalProperties:

 $ref: 'TS29571\_CommonData.yaml#/components/schemas/PresenceInfo'

 minProperties: 0

 required:

 - locationReportingMessageType N2ConnectionMessageType:

 type: integer

 LocationReportingMessageType:

 type: integer

 NotificationType:

 anyOf:

 - type: string

 enum:

 - REAUTHORIZATION

 - ABORT\_CHARGING

 - type: string

 NodeFunctionality:

 anyOf:

 - type: string

 enum:

 - AMF

 - SMF

 - SMSF

 - SGW

 - I\_SMF

 - CEF

 - type: string

 ChargingCharacteristicsSelectionMode:

 anyOf:

 - type: string

 enum:

 - HOME\_DEFAULT

 - ROAMING\_DEFAULT

 - VISITING\_DEFAULT

 - type: string

 TriggerType:

 anyOf:

 - type: string

 enum:

 - QUOTA\_THRESHOLD

 - QHT

 - FINAL

 - QUOTA\_EXHAUSTED

 - VALIDITY\_TIME

 - OTHER\_QUOTA\_TYPE

 - FORCED\_REAUTHORISATION

 - UNUSED\_QUOTA\_TIMER # Included for backwards compatibility, shall not be used

 - UNIT\_COUNT\_INACTIVITY\_TIMER

 - ABNORMAL\_RELEASE

 - QOS\_CHANGE

 - VOLUME\_LIMIT

 - TIME\_LIMIT

 - EVENT\_LIMIT

 - PLMN\_CHANGE

 - USER\_LOCATION\_CHANGE

 - RAT\_CHANGE

 - SESSION\_AMBR\_CHANGE

 - UE\_TIMEZONE\_CHANGE

 - TARIFF\_TIME\_CHANGE

 - MAX\_NUMBER\_OF\_CHANGES\_IN\_CHARGING\_CONDITIONS

 - MANAGEMENT\_INTERVENTION

 - CHANGE\_OF\_UE\_PRESENCE\_IN\_PRESENCE\_REPORTING\_AREA

 - CHANGE\_OF\_3GPP\_PS\_DATA\_OFF\_STATUS

 - SERVING\_NODE\_CHANGE

 - REMOVAL\_OF\_UPF

 - ADDITION\_OF\_UPF

 - INSERTION\_OF\_ISMF

 - REMOVAL\_OF\_ISMF

 - CHANGE\_OF\_ISMF

 - START\_OF\_SERVICE\_DATA\_FLOW

 - ECGI\_CHANGE

 - TAI\_CHANGE

 - HANDOVER\_CANCEL

 - HANDOVER\_START

 - HANDOVER\_COMPLETE

 - GFBR\_GUARANTEED\_STATUS\_CHANGE

 - type: string

 FinalUnitAction:

 anyOf:

 - type: string

 enum:

 - TERMINATE

 - REDIRECT

 - RESTRICT\_ACCESS

 - type: string

 RedirectAddressType:

 anyOf:

 - type: string

 enum:

 - IPV4

 - IPV6

 - URL

 - type: string

 TriggerCategory:

 anyOf:

 - type: string

 enum:

 - IMMEDIATE\_REPORT

 - DEFERRED\_REPORT

 - type: string

 QuotaManagementIndicator:

 anyOf:

 - type: string

 enum:

 - ONLINE\_CHARGING

 - OFFLINE\_CHARGING

 - type: string

 FailureHandling:

 anyOf:

 - type: string

 enum:

 - TERMINATE

 - CONTINUE

 - RETRY\_AND\_TERMINATE

 - type: string

 SessionFailover:

 anyOf:

 - type: string

 enum:

 - FAILOVER\_NOT\_SUPPORTED

 - FAILOVER\_SUPPORTED

 - type: string

 3GPPPSDataOffStatus:

 anyOf:

 - type: string

 enum:

 - ACTIVE

 - INACTIVE

 - type: string

 ResultCode:

 anyOf:

 - type: string

 enum:

 - SUCCESS

 - END\_USER\_SERVICE\_DENIED

 - QUOTA\_MANAGEMENT\_NOT\_APPLICABLE

 - QUOTA\_LIMIT\_REACHED

 - END\_USER\_SERVICE\_REJECTED

 - USER\_UNKNOWN

 - RATING\_FAILED

 - type: string

 PartialRecordMethod:

 anyOf:

 - type: string

 enum:

 - DEFAULT

 - INDIVIDUAL

 - type: string

 RoamerInOut:

 anyOf:

 - type: string

 enum:

 - IN\_BOUND

 - OUT\_BOUND

 - type: string

 SMMessageType:

 anyOf:

 - type: string

 enum:

 - SUBMISSION

 - DELIVERY\_REPORT

 - SM\_SERVICE\_REQUEST

 - type: string

 SMPriority:

 anyOf:

 - type: string

 enum:

 - LOW

 - NORMAL

 - HIGH

 - type: string

 DeliveryReportRequested:

 anyOf:

 - type: string

 enum:

 - YES

 - NO

 - type: string

 InterfaceType:

 anyOf:

 - type: string

 enum:

 - UNKNOWN

 - MOBILE\_ORIGINATING

 - MOBILE\_TERMINATING

 - APPLICATION\_ORIGINATING

 - APPLICATION\_TERMINATING

 - type: string

 ClassIdentifier:

 anyOf:

 - type: string

 enum:

 - PERSONAL

 - ADVERTISEMENT

 - INFORMATIONAL

 - AUTO

 - type: string

 SMAddressType:

 anyOf:

 - type: string

 enum:

 - EMAIL\_ADDRESS

 - MSISDN

 - IPV4\_ADDRESS

 - IPV6\_ADDRESS

 - NUMERIC\_SHORTCODE

 - ALPHANUMERIC\_SHORTCODE

 - OTHER

 - IMSI

 - type: string

 SMAddresseeType:

 anyOf:

 - type: string

 enum:

 - TO

 - CC

 - BCC

 - type: string

 SMServiceType:

 anyOf:

 - type: string

 enum:

 - VAS4SMS\_SHORT\_MESSAGE\_CONTENT\_PROCESSING

 - VAS4SMS\_SHORT\_MESSAGE\_FORWARDING

 - VAS4SMS\_SHORT\_MESSAGE\_FORWARDING\_MULTIPLE\_SUBSCRIPTIONS

 - VAS4SMS\_SHORT\_MESSAGE\_FILTERING

 - VAS4SMS\_SHORT\_MESSAGE\_RECEIPT

 - VAS4SMS\_SHORT\_MESSAGE\_NETWORK\_STORAGE

 - VAS4SMS\_SHORT\_MESSAGE\_TO\_MULTIPLE\_DESTINATIONS

 - VAS4SMS\_SHORT\_MESSAGE\_VIRTUAL\_PRIVATE\_NETWORK(VPN)

 - VAS4SMS\_SHORT\_MESSAGE\_AUTO\_REPLY

 - VAS4SMS\_SHORT\_MESSAGE\_PERSONAL\_SIGNATURE

 - VAS4SMS\_SHORT\_MESSAGE\_DEFERRED\_DELIVERY

 - type: string

 ReplyPathRequested:

 anyOf:

 - type: string

 enum:

 - NO\_REPLY\_PATH\_SET

 - REPLY\_PATH\_SET

 - type: string

 oneTimeEventType:

 anyOf:

 - type: string

 enum:

 - IEC

 - PEC

 - type: string

 dnnSelectionMode:

 anyOf:

 - type: string

 enum:

 - VERIFIED

 - UE\_DNN\_NOT\_VERIFIED

 - NW\_DNN\_NOT\_VERIFIED

 - type: string

 APIDirection:

 anyOf:

 - type: string

 enum:

 - INVOCATION

 - NOTIFICATION

 - type: string

 RegistrationMessageType:

 anyOf:

 - type: string

 enum:

 - INITIAL

 - MOBILITY

 - PERIODIC

 - EMERGENCY

 - DEREGISTRATION

 - type: string

 MICOModeIndication:

 anyOf:

 - type: string

 enum:

 - MICO\_MODE

 - NO\_MICO\_MODE

 - type: string

 SmsIndication:

 anyOf:

 - type: string

 enum:

 - SMS\_SUPPORTED

 - SMS\_NOT\_SUPPORTED

 - type: string

|  |
| --- |
| **End of change** |