- No.: 2
- Timestamp: 10:51:55:904_0
- RFN: 3196
- Chip: 14080
- Event: Start Timer
- Source: tc_7_2_3_19 LINE 1
- Message Structure:
no details available
- Constraint:
t_Guard (300 Sec)
- BinaryMessage:

- No.: 88
- Timestamp: 10:51:55:937_0
- RFN: 3199
- Chip: 25600
- Event: Send
- PCO: Ut
- Message: MMI_CmdReq
- Source: ts_MMI_UE_SwitchOff LINE 1
- Message Structure:
MMI_CmdReq
. (IA5StringType)cmd[-1] = "Please switch off the UE"
- Constraint:
ca_MMI_CmdReq
- BinaryMessage:
50 6c 65 61 73 65 20 73 77 69 74 63 68 20 6f 66 66 20 20 74 68 65 20 55 45

- No.: 92
- Timestamp: 10:51:58:122_0
- RFN: 3418
- Chip: 5888
- Event: Receive
- PCO: Ut
- Message: MMI_CmdCnf
- Source: ts_MMI_UE_SwitchOff LINE 2
- Message Structure:
MMI_CmdCnf
. (BooleanType)result = TRUE
. (IA5StringType)resultString[6] = " OK "
- Constraint:
ca_MMI_CmdCnf
- BinaryMessage:
80 0d 0a 4f 4b 0d 0a

- No.: 96
- Timestamp: 10:51:58:125_0
- RFN: 3418
- Chip: 18944
- Event: Send
- PCO: CPHY
- Message: CPHY_Ini_REQ
- Source: ts_SS_CellCfg:lt_CelllsAlreadyStarted LINE 5
- Message Structure:
CPHY_Ini_REQ
. (CPHY_Ini_REQ)CPHY_Ini_REQ = 0
- Constraint:
cas_InitReqDef
- BinaryMessage:
0a 01 00

- No.: 100
- Timestamp: 10:52:00:169_0
- RFN: 10
- Chip: 14080
- Event: Receive
- PCO: CPHY
- Message: CPHY_Ini_CNF
- Source: ts_SS_CellCfg:lt_CelllsAlreadyStarted LINE 6
- Message Structure:
CPHY_Ini_CNF
- Constraint:
car_IniCnf
- BinaryMessage:
30 02 05 00

- No.: 104
- Timestamp: 10:52:00:172_0
- RFN: 10
- Chip: 26368
- Event: Send
- PCO: CPHY
- Message: CPHY_Cell_Config_REQ
- Source: ts_SS_CellCfg LINE 6
- Message Structure:
CPHY_Cell_Config_REQ
. (IntegerType)cellId = 0
. (IntegerType)tcell = 0
. (IntegerType)sfnOffset = 0
. FrequencyInfo
. . modeSpecificInfo
. . . FrequencyInfoFDD
. . . . (IntegerType)uarfcn_UL = -
. . . . (IntegerType)uarfcn_DL = 10700
. (IntegerType)primaryScramblingCode_SS = 100
. CellTxPowerLevel
. (IntegerType)dLTxAttenuationLevel = 0
- Constraint:
ca_CellCfgReq
- BinaryMessage:
30 19 02 01 00 02 01 00 02 01 00 30 06 30 04 02 02 29 cc 02 01 64 05 00 02 01 00

- No.: 108
- Timestamp: 10:52:01:085_0
- RFN: 101
- Chip: 38144
- Event: Receive
- PCO: CPHY
- Message: CPHY_Cell_Config_CNF
- Source: ts_SS_CellCfg LINE 7
- Message Structure:
CPHY_Cell_Config_CNF
. (IntegerType)cellId = 0
- Constraint:
ca_CellCfgCnf
- BinaryMessage:
30 03 02 01 00

- No.: 120
- Timestamp: 10:52:01:092_0
- RFN: 102
- Chip: 25088
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 3
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 0
. (RatType)ratType = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . PrimaryCPICHInfo
. . . . (IntegerType)dl_TxPower_PCPICH = -60
. . . . (BooleanType)txdiversityIndicator = FALSE
- Constraint:
ca_pCPICH_Info
- BinaryMessage:
30 13 02 01 00 02 01 00 0a 01 00 30 08 30 06 02 01 c4 01 01 00

- No.: 124
- Timestamp: 10:52:01:098_0
- RFN: 103
- Chip: 7936
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 4
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 0
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 00

- No.: 125
- Timestamp: 10:52:01:101_0
- RFN: 103
- Chip: 21248
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 5
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 1
. (RatType)ratType = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . PrimarySCHInfo
. . . . (BooleanType)tstdIndicator = FALSE
. . . . (IntegerType)dl_TxPower = -5
- Constraint:
ca_pSCH_Info
- BinaryMessage:
30 13 02 01 00 02 01 01 0a 01 00 30 08 30 06 01 01 00 02 01 fb

- No.: 129
- Timestamp: 10:52:01:106_0
- RFN: 104
- Chip: 2048
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 6
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 1
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 01

- No.: 130
- Timestamp: 10:52:01:109_0
- RFN: 104
- Chip: 15104
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 7
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 2
. (RatType)ratType = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . SecondarySCHInfo
. . . . (BooleanType)tstdIndicator = FALSE
. . . . (IntegerType)dl_TxPower = -5
- Constraint:
ca_sSCH_Info
- BinaryMessage:
30 13 02 01 00 02 01 02 0a 01 00 30 08 30 06 01 01 00 02 01 fb

- No.: 134
- Timestamp: 10:52:01:248_0
- RFN: 118
- Chip: 7936
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 8
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 2
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 02

- No.: 135
- Timestamp: 10:52:01:252_0
- RFN: 118
- Chip: 22016
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 9
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 4
. (RatType)ratType = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . PrimaryCCPCHInfo
. . . . (BooleanType)sttd_Indicator = FALSE
. . . . (IntegerType)dl_TxPower = -2
- Constraint:
ca_pCCPCH_Info
- BinaryMessage:
30 13 02 01 00 02 01 04 0a 01 00 30 08 30 06 01 01 00 02 01 fe

- No.: 139
- Timestamp: 10:52:01:259_0
- RFN: 119
- Chip: 11008
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 10
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 4
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 04

- No.: 140
- Timestamp: 10:52:01:270_0
- RFN: 120
- Chip: 14336
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Config_REQ
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 11
- Message Structure:
CPHY_TrCH_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 4
. (RatType)ratType = 0
. CphyTrchConfigReq
. . SS_ActivationTime
. . ulconnectedTrCHList
. . TFCS
. . dlconnectedTrCHList
. . . CphyTrchConfigReq_setseq_1
. . . . (IntegerType)trchid = 11
. . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 2
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 246
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional = 0
. . . . . . (IntegerType)rateMatchingAttribute = 1
. . . . . . (CRC_Size)crc_Size = 3
. . TFCS
. . . ExplicitTFCS_Configuration
. . . . TFCS_ReconfAdd
. . . . . ctfcSize
. . . . . . ctfc2Bit
. . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . (IntegerType)ctfc2 = 0
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . fdd
. . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 11
. . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
- Constraint:
ca_BCH_InfoActNow
- BinaryMessage:
30 4c 02 01 00 02 01 04 0a 01 00 30 41 05 00 30 23 30 21 02 01 0b 0a 01 02 30 19 30 0c 30 0a 02 02 00 f6 30 02 05 00 05 00 30 09 0a 01 00 02 01 01 0a 01 03 30 18 30 30 15 30 13 02 01 00 30 0e 30 0c 30 30 03 02 01 0b 02 01 0f 02 01 00

- No.: 144
- Timestamp: 10:52:01:277_0
- RFN: 121
- Chip: 5376
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Config_CNF
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 12
- Message Structure:
CPHY_TrCH_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 4
- Constraint:
ca_TrChCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 04

- No.: 145
- Timestamp: 10:52:01:293_0
- RFN: 122
- Chip: 28160
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 13
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 4
. (RatType)ratType = 0
. configMessage
. . CmacConfigReq
. . . SS_ActivationTime
. . . UE_Info
. . . . U_RNTI
. . . . (BitStringType)c_RNTI[16] = -
. . . TrCHInfo
. . . . ulconnectedTrCHList
. . . . TFCS
. . . . dlconnectedTrCHList
. . . . . TrCHInfo_setseq_1
. . . . . . (IntegerType)trchid = 11
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 246
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional = 0
. . . . . . . . (IntegerType)rateMatchingAttribute = 1
. . . . . . . . (CRC_Size)crc_Size = 3
. . . . TFCS
. . . . . ExplicitTFCS_Configuration
. . . . . . TFCS_ReconfAdd
. . . . . . . ctfcSize
. . . . . . . . ctfc2Bit
. . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . (IntegerType)ctfc2 = 0
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 11
. . . . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . TrCH_LogCHMappingList1
. . . . ulconnectedTrCHList
. . . . dlconnectedTrCHList
. . . . . TrCH_LogCHMappingList1_setseq_1
. . . . . . (IntegerType)trchid = 11
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 2
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 0
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 1
. . . . . . . . (IntegerType)rB_Identity = -1
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_CMAC_CfgInfo
- BinaryMessage:
30 70 02 01 00 02 01 04 0a 01 00 30 65 05 00 30 00 30 3c 30 20 30 1e 02 01 0b 30 19 30 0c 30 0a 02 02 00 f6 30 02 05 00 05 00 30 09 0a 01 00 02 01 01 0a 01 03 30 18 30 30 15 30 13 02 01 00 30 0e 30 0c 30 30 03 02 01 0b 02 01 0f 02 01 00 30 21 30 1f 30 1d 02 01 0b 30 18 30 16 30 11 0a 01 00 0a 01 02 02 01 01 0a 01 00 05 00 02 01 01 02 01 ff

- No.: 149
- Timestamp: 10:52:01:304_0
- RFN: 123
- Chip: 31232
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 14
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 4
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 04

- No.: 157
- Timestamp: 10:52:01:310_0
- RFN: 124
- Chip: 15872
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_PCH_FACH_CCCH_Cfg LINE 3
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 5
. (RatType)ratType = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . SecondaryCCPCHInfo
. . . . (IntegerType)scramblingCode = 0
. . . . SF256_AndCodeNumber
. . . . . (IntegerType)sf64 = 1
. . . . (IntegerType)sCCPCHSlotFormat = 8
. . . . (IntegerType)timingOffset = 0
. . . . (PositionFixedOrFlexible)positionFixedOrFlexible = 1
. . . . (BooleanType)sttd_Indicator = FALSE
. . . . (IntegerType)dl_TxPower = -2
. . . . (IntegerType)powerOffsetOfTFCI_PO1 = 6
. . . . (IntegerType)powerOffsetOfPILOT_PO3 = 6
- Constraint:
ca_sCCPCH_Info
- BinaryMessage:
30 28 02 01 00 02 01 05 0a 01 00 30 1d 30 1b 02 01 00 02 01 01 02 01 08 02 01 00 0a 01 01 01 01 00 02 01 fe 02 01 06 02 01 06

- No.: 161
- Timestamp: 10:52:01:317_0
- RFN: 125
- Chip: 4352
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_PCH_FACH_CCCH_Cfg LINE 4
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 5
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 05

- No.: 162
- Timestamp: 10:52:01:343_0
- RFN: 127
- Chip: 26880
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Config_REQ
- Source: ts_SS_PCH_FACH_CCCH_Cfg LINE 5
- Message Structure:
CPHY_TrCH_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 5
. (RatType)ratType = 0
. CphyTrchConfigReq
. . SS_ActivationTime
. . ulconnectedTrCHList
. . TFCS
. . dlconnectedTrCHList
. . . CphyTrchConfigReq_setseq_1
. . . . (IntegerType)trchid = 12
. . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 3
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 240
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional = 0
. . . . . . (IntegerType)rateMatchingAttribute = 230
. . . . . . (CRC_Size)crc_Size = 3
. . . CphyTrchConfigReq_setseq_1
. . . . (IntegerType)trchid = 13
. . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 1
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 168
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . (IntegerType)small = 2
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional = 0
. . . . . . (IntegerType)rateMatchingAttribute = 220
. . . . . . (CRC_Size)crc_Size = 3
. . . CphyTrchConfigReq_setseq_1
. . . . (IntegerType)trchid = 14
. . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 1
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 360
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . (IntegerType)rateMatchingAttribute = 130
. . . . . . (CRC_Size)crc_Size = 3
. . TFCS
. . . ExplicitTFCS_Configuration
. . . . TFCS_ReconfAdd
. . . . . ctfcSize
. . . . . . ctfc4Bit
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 0
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 1
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 2
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 3
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 4
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 5
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 6
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 8
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . fdd
. . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 11
. . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
- Constraint:
ca_PCH_2_FACH_InfoActNow
- BinaryMessage:
30 81 e4 02 01 00 02 01 05 0a 01 00 30 81 d8 05 00 30 74 30 24 02 01 0c 0a 01 03 30 1c 30 0e 30 0c 02 02 00 f0 30 04 05 00 05 00 05 00 30 0a 0a 01 00 02 02 00 e6 0a 01 03 30 27 02 01 0d 0a 01 01 30 1f 30 11 30 0f 02 02 00 a8 30 07 05 00 05 00 02 01 02 05 00 30 0a 0a 01 00 02 02 00 dc 0a 01 03 30 23 02 01 0e 0a 01 01 30 1b 30 0e 30 0c 02 02 01 68 30 04 05 00 05 00 05 00 30 09 05 00 02 02 00 82 0a 01 03 30 5e 30 30 5b 30 08 02 01 00 30 03 02 01 00 30 08 02 01 01 30 03 02 01 00 30 08 02 01 02 30 03 02 01 00 30 08 02 01 03 30 03 02 01 00 30 08 02 01 04 30 03 02 01 00 30 08 02 01 05 30 03 02 01 00 30 08 02 01 06 30 03 02 01 00 30 13 02 01 08 30 0e 30 0c 30 30 03 02 01 0b 02 01 0f 02 01 00

- No.: 166
- Timestamp: 10:52:01:354_0
- RFN: 128
- Chip: 30464
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Config_CNF
- Source: ts_SS_PCH_FACH_CCCH_Cfg LINE 6
- Message Structure:
CPHY_TrCH_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 5
- Constraint:
ca_TrChCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 05

- No.: 167
- Timestamp: 10:52:01:393_0
- RFN: 132
- Chip: 29696
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_SS_PCH_FACH_CCCH_Cfg LINE 7
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 5
. (RatType)ratType = 0
. configMessage
. . CmacConfigReq
. . . SS_ActivationTime
. . . UE_Info
. . . . U_RNTI
. . . . (BitStringType)c_RNTI[16] = -
. . . TrCHInfo
. . . . ulconnectedTrCHList
. . . . TFCS
. . . . dlconnectedTrCHList
. . . . . TrCHInfo_setseq_1
. . . . . . (IntegerType)trchid = 12
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 240
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional = 0
. . . . . . . . (IntegerType)rateMatchingAttribute = 230
. . . . . . . . (CRC_Size)crc_Size = 3
. . . . . TrCHInfo_setseq_1
. . . . . . (IntegerType)trchid = 13
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 168
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . (IntegerType)small = 2
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional = 0
. . . . . . . . (IntegerType)rateMatchingAttribute = 220
. . . . . . . . (CRC_Size)crc_Size = 3
. . . . . TrCHInfo_setseq_1
. . . . . . (IntegerType)trchid = 14
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 360
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . (IntegerType)rateMatchingAttribute = 130
. . . . . . . . (CRC_Size)crc_Size = 3
. . . . TFCS
. . . . . ExplicitTFCS_Configuration
. . . . . . TFCS_ReconfAdd
. . . . . . . ctfcSize
. . . . . . . . ctfc4Bit
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 0
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 1
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 2
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 3
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 4
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 5
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 6
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 8
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 11
. . . . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . TrCH_LogCHMappingList1
. . . . ulconnectedTrCHList
. . . . dlconnectedTrCHList
. . . . . TrCH_LogCHMappingList1_setseq_1
. . . . . . (IntegerType)trchid = 12
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 3
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 1
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 1
. . . . . . . . (IntegerType)rB_Identity = -2
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . TrCH_LogCHMappingList1_setseq_1
. . . . . . (IntegerType)trchid = 13
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 1
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 5
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 2
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 1
. . . . . . . . (IntegerType)rB_Identity = 0
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_CMAC_CfgInfo
- BinaryMessage:
30 82 01 23 02 01 00 02 01 05 0a 01 00 30 82 01 16 05 00 30 00 30 81 cd 30 6b 30 21 02 01 0c 30 1c 30 0e 30 0c 02 02 00 f0 30 04 05 00 05 00 05 00 30 0a 0a 01 00 02 02 00 e6 0a 01 03 30 24 02 01 0d 30 1f 30 11 30 0f 02 02 00 a8 30 07 05 00 05 00 02 01 02 05 00 30 0a 0a 01 00 02 02 00 dc 0a 01 03 30 20 02 01 0e 30 1b 30 0e 30 0c 02 02 01 68 30 04 05 00 05 00 05 00 30 09 05 00 02 02 00 82 0a 01 03 30 5e 30 30 5b 30 08 02 01 00 30 03 02 01 00 30 08 02 01 01 30 03 02 01 00 30 08 02 01 02 30 03 02 01 00 30 08 02 01 03 30 03 02 01 00 30 08 02 01 04 30 03 02 01 00 30 08 02 01 05 30 03 02 01 00 30 08 02 01 06 30 03 02 01 00 30 13 02 01 08 30 0e 30 0c 30 30 03 02 01 0b 02 01 0f 02 01 00 30 40 30 3e 30 1d 02 01 0c 30 18 30 16 30 11 0a 01 00 0a 01 03 02 01 01 0a 01 01 05 00 02 01 01 02 01 fe 30 1d 02 01 0d 30 18 30 16 30 11 0a 01 00 0a 01 01 02 01 05 0a 01 02 05 00 02 01 01 02 01 00

- No.: 171
- Timestamp: 10:52:01:441_0
- RFN: 137
- Chip: 23552
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_SS_PCH_FACH_CCCH_Cfg LINE 8
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 5
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 05

- No.: 172
- Timestamp: 10:52:01:446_0
- RFN: 138
- Chip: 2304
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_PCH_FACH_CCCH_Cfg LINE 9
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 6
. (RatType)ratType = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . PICHInfo
. . . . PICH_Info
. . . . . fdd
. . . . . . (IntegerType)channelisationCode256 = 2
. . . . . . (PI_CountPerFrame)pi_CountPerFrame = 0
. . . . . . (BooleanType)sttd_Indicator = FALSE
. . . . (IntegerType)dl_TxPower = -5
- Constraint:
ca_PICH_Info
- BinaryMessage:
30 1c 02 01 00 02 01 06 0a 01 00 30 11 30 0f 30 30 09 02 01 02 0a 01 00 01 01 00 02 01 fb

- No.: 176
- Timestamp: 10:52:01:453_0
- RFN: 138
- Chip: 30464
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_PCH_FACH_CCCH_Cfg LINE 10
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 6
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 06

- No.: 184
- Timestamp: 10:52:01:459_0
- RFN: 139
- Chip: 14336
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_RACH_CCCH_Cfg LINE 3
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 7
. (RatType)ratType = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . AICHInfo
. . . . AICH_Info
. . . . . (IntegerType)channelisationCode256 = 3
. . . . . (BooleanType)sttd_Indicator = FALSE
. . . . . (AICH_TransmissionTiming)aich_TransmissionTiming = 0
. . . . (IntegerType)dl_TxPower = -5
- Constraint:
ca_AichInfo
- BinaryMessage:
30 1b 02 01 00 02 01 07 0a 01 00 30 10 30 0e 30 09 02 01 03 01 01 00 0a 01 00 02 01 fb

- No.: 188
- Timestamp: 10:52:01:468_0
- RFN: 140
- Chip: 6144
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_RACH_CCCH_Cfg LINE 4
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 7
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 07

- No.: 189
- Timestamp: 10:52:01:473_0
- RFN: 140
- Chip: 24064
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_RACH_CCCH_Cfg LINE 5
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 8
. (RatType)ratType = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . PRACHInfo
. . . . fdd_tdd
. . . . . fdd
. . . . . . (BitStringType)preambleSignature[16] = "0000000011111111"
. . . . . . (SF_PRACH)spreadingFactorForDataPart = 1
. . . . . . (IntegerType)preambleScramblingCode = 0
. . . . . . (PuncturingLimit)puncturingLimit = 15
. . . . . . (BitStringType)accessSlot[12] = "111111111111"
- Constraint:
ca_PRACH_Info
- BinaryMessage:
30 23 02 01 00 02 01 08 0a 01 00 30 18 30 16 30 30 13 03 03 00 00 ff 0a 01 01 02 01 00 0a 01 0f 03 03 04 ff f0

- No.: 193
- Timestamp: 10:52:01:482_0
- RFN: 141
- Chip: 23040
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_RACH_CCCH_Cfg LINE 6
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 8
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 08

- No.: 194
- Timestamp: 10:52:01:494_0
- RFN: 142
- Chip: 28160
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Config_REQ
- Source: ts_SS_RACH_CCCH_Cfg LINE 7
- Message Structure:
CPHY_TrCH_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 8
. (RatType)ratType = 0
. CphyTrchConfigReq
. . SS_ActivationTime
. . ulconnectedTrCHList
. . . CphyTrchConfigReq_setseq_0
. . . . (IntegerType)trchid = 15
. . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 1
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 168
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 360
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional = 0
. . . . . . (IntegerType)rateMatchingAttribute = 150
. . . . . . (CRC_Size)crc_Size = 3
. . TFCS
. . . ExplicitTFCS_Configuration
. . . . TFCS_ReconfAdd
. . . . . ctfcSize
. . . . . . ctfc2Bit
. . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . (IntegerType)ctfc2 = 0
. . . . . . . . PowerOffsetInformation
. . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . (IntegerType)ctfc2 = 1
. . . . . . . . PowerOffsetInformation
. . dlconnectedTrCHList
. . TFCS
- Constraint:
cab_RACH_InfoActNow
- BinaryMessage:
30 4e 02 01 00 02 01 08 0a 01 00 30 43 05 00 30 30 30 2e 02 01 0f 0a 01 01 30 26 30 18 30 0a 02 02 00 a8 30 02 05 00 05 00 30 0a 02 02 01 68 30 02 05 00 05 00 30 0a 0a 01 00 02 02 00 96 0a 01 03 30 0d 30 30 0a 30 03 02 01 00 30 03 02 01 01

- No.: 198
- Timestamp: 10:52:01:503_0
- RFN: 143
- Chip: 27392
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Config_CNF
- Source: ts_SS_RACH_CCCH_Cfg LINE 8
- Message Structure:
CPHY_TrCH_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 8
- Constraint:
ca_TrChCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 08

- No.: 199
- Timestamp: 10:52:01:522_0
- RFN: 145
- Chip: 20736
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_SS_RACH_CCCH_Cfg LINE 9
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 8
. (RatType)ratType = 0
. configMessage
. . CmacConfigReq
. . . SS_ActivationTime
. . . UE_Info
. . . . U_RNTI
. . . . (BitStringType)c_RNTI[16] = -
. . . TrCHInfo
. . . . ulconnectedTrCHList
. . . . . TrCHInfo_setseq_0
. . . . . . (IntegerType)trchid = 15
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 168
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 360
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional = 0
. . . . . . . . (IntegerType)rateMatchingAttribute = 150
. . . . . . . . (CRC_Size)crc_Size = 3
. . . . TFCS
. . . . . ExplicitTFCS_Configuration
. . . . . . TFCS_ReconfAdd
. . . . . . . ctfcSize
. . . . . . . . ctfc2Bit
. . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . (IntegerType)ctfc2 = 0
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . (IntegerType)ctfc2 = 1
. . . . . . . . . . PowerOffsetInformation
. . . . dlconnectedTrCHList
. . . . TFCS
. . . TrCH_LogCHMappingList1
. . . . ulconnectedTrCHList
. . . . . TrCH_LogCHMappingList1_setseq_0
. . . . . . (IntegerType)trchid = 15
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 1
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 5
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 2
. . . . . . . . (IntegerType)rB_Identity = 0
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . dlconnectedTrCHList
- Constraint:
ca_CMAC_CfgInfo
- BinaryMessage:
30 6d 02 01 00 02 01 08 0a 01 00 30 62 05 00 30 00 30 3e 30 2d 30 2b 02 01 0f 30 26 30 18 30 0a 02 02 00 a8 30 02 05 00 05 00 30 0a 02 02 01 68 30 02 05 00 05 00 30 0a 0a 01 00 02 02 00 96 0a 01 03 30 0d 30 30 0a 30 03 02 01 00 30 03 02 01 01 30 1c 30 1a 30 18 02 01 0f 30 13 30 11 30 0c 0a 01 00 0a 01 01 02 01 05 0a 01 02 02 01 00

- No.: 203
- Timestamp: 10:52:01:529_0
- RFN: 146
- Chip: 9728
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_SS_RACH_CCCH_Cfg LINE 10
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 8
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 08

- No.: 240
- Timestamp: 10:52:01:548_0
- RFN: 148
- Chip: 6400
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_1DCH_DCCH_Cfg LINE 4
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
. (RatType)ratType = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . DPCHInfo
. . . . UL_DPCH_Info
. . . . DL_DPCHInfo
. . . . . DL_CommonInformation
. . . . . . DL_DPCH_InfoCommon
. . . . . . . cfnHandling
. . . . . . . . initialise
. . . . . . . . . (IntegerType)cfntargetsfnframeoffset = -
. . . . . . . modeSpecificInfo
. . . . . . . . fdd
. . . . . . . . . DL_DPCH_PowerControlInfo
. . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . fdd
. . . . . . . . . . . . (DPC_Mode)dpc_Mode = 0
. . . . . . . . . (IntegerType)powerOffsetPilot_pdpdch = 0
. . . . . . . . . Dl_rate_matching_restriction
. . . . . . . . . SF512_AndPilot
. . . . . . . . . . (PilotBits128)sfd128 = 0
. . . . . . . . . (PositionFixedOrFlexible)positionFixedOrFlexible = 0
. . . . . . . . . (BooleanType)tfci_Existence = FALSE
. . . . . . modeSpecificInfo
. . . . . . . fdd
. . . . . . . . (IntegerType)defaultDPCH_OffsetValue = 0
. . . . . . . . DPCH_CompressedModeInfo
. . . . . . . . (TX_DiversityMode)tx_DiversityMode = 0
. . . . . . . . SSDT_Information
. . . . . DL_DPCH_InfoPerRL
. . . . . . fdd
. . . . . . . (PCPICH_UsageForChannelEst)pCPICH_UsageForChannelEst = 0
. . . . . . . (IntegerType)dpch_FrameOffset = 0
. . . . . . . SecondaryCPICH_Info
. . . . . . . DL_ChannelisationCodeList
. . . . . . . . DL_ChannelisationCode
. . . . . . . . . (IntegerType)secondaryScramblingCode = 1
. . . . . . . . . SF512_AndCodeNumber
. . . . . . . . . . (IntegerType)sf128 = 0
. . . . . . . . . (ScramblingCodeChange)scramblingCodeChange = -
. . . . . . . (IntegerType)tpc_CombinationIndex = 0
. . . . . . . (SSDT_CellIdentity)ssdt_CellIdentity = -
. . . . . . . (ClosedLoopTimingAdjMode)closedLoopTimingAdjMode = -
. . . . . (IntegerType)powerOffsetOfTFCI_PO1 = 0
. . . . . (IntegerType)powerOffsetOfTPC_PO2 = 0
. . . . . (IntegerType)powerOffsetOfPILOT_PO3 = 0
. . . . . (IntegerType)dl_TxPower = -5
. . . . . (IntegerType)dl_TxPowerMax = 15
. . . . . (IntegerType)dl_TxPowerMin = -35
- Constraint:
ca_DL_DPCH_Info
- BinaryMessage:
30 5e 02 01 00 02 01 1a 0a 01 00 30 53 30 51 30 4f 30 25 30 1a 30 30 00 30 30 14 30 06 30 30 03 0a 01 00 02 01 00 0a 01 00 0a 01 00 01 01 00 30 30 06 02 01 00 0a 01 00 30 30 13 0a 01 00 02 01 00 30 08 30 06 02 01 01 02 01 00 02 01 00 02 01 00 02 01 00 02 01 00 02 01 fb 02 01 0f 02 01 dd

- No.: 244
- Timestamp: 10:52:01:555_0
- RFN: 148
- Chip: 35840
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_1DCH_DCCH_Cfg LINE 5
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 1a

- No.: 245
- Timestamp: 10:52:01:567_0
- RFN: 150
- Chip: 5376
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Config_REQ
- Source: ts_SS_1DCH_DCCH_Cfg LINE 6
- Message Structure:
CPHY_TrCH_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
. (RatType)ratType = 0
. CphyTrchConfigReq
. . SS_ActivationTime
. . ulconnectedTrCHList
. . TFCS
. . dlconnectedTrCHList
. . . CphyTrchConfigReq_setseq_1
. . . . (IntegerType)trchid = 10
. . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 148
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional = 1
. . . . . . (IntegerType)rateMatchingAttribute = 192
. . . . . . (CRC_Size)crc_Size = 3
. . TFCS
. . . ExplicitTFCS_Configuration
. . . . TFCS_ReconfAdd
. . . . . ctfcSize
. . . . . . ctfc2Bit
. . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . (IntegerType)ctfc2 = 0
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . (IntegerType)ctfc2 = 1
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . fdd
. . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 11
. . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
- Constraint:
ca_DCH_148_TTI_10_DL_InfoActNow
- BinaryMessage:
30 59 02 01 00 02 01 1a 0a 01 00 30 4e 05 00 30 26 30 24 02 01 0a 0a 01 00 30 1c 30 0e 30 0c 02 02 00 94 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 c0 0a 01 03 30 22 30 30 1f 30 08 02 01 00 30 03 02 01 00 30 13 02 01 01 30 0e 30 0c 30 30 03 02 01 0b 02 01 0f 02 01 00

- No.: 249
- Timestamp: 10:52:01:576_0
- RFN: 150
- Chip: 37120
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Config_CNF
- Source: ts_SS_1DCH_DCCH_Cfg LINE 7
- Message Structure:
CPHY_TrCH_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
ca_TrChCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 1a

- No.: 250
- Timestamp: 10:52:01:609_0
- RFN: 154
- Chip: 11264
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_SS_1DCH_DCCH_Cfg LINE 8
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
. (RatType)ratType = 0
. configMessage
. . CmacConfigReq
. . . SS_ActivationTime
. . . UE_Info
. . . . U_RNTI
. . . . (BitStringType)c_RNTI[16] = -
. . . TrCHInfo
. . . . ulconnectedTrCHList
. . . . TFCS
. . . . dlconnectedTrCHList
. . . . . TrCHInfo_setseq_1
. . . . . . (IntegerType)trchid = 10
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 148
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . (IntegerType)rateMatchingAttribute = 192
. . . . . . . . (CRC_Size)crc_Size = 3
. . . . TFCS
. . . . . ExplicitTFCS_Configuration
. . . . . . TFCS_ReconfAdd
. . . . . . . ctfcSize
. . . . . . . . ctfc2Bit
. . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . (IntegerType)ctfc2 = 0
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . (IntegerType)ctfc2 = 1
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 11
. . . . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . TrCH_LogCHMappingList1
. . . . ulconnectedTrCHList
. . . . dlconnectedTrCHList
. . . . . TrCH_LogCHMappingList1_setseq_1
. . . . . . (IntegerType)trchid = 10
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 1
. . . . . . . . (IntegerType)rB_Identity = 1
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 2
. . . . . . . . (IntegerType)rB_Identity = 2
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 3
. . . . . . . . (IntegerType)rB_Identity = 3
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 4
. . . . . . . . (IntegerType)rB_Identity = 4
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_CMAC_CfgInfo
- BinaryMessage:
30 81 c6 02 01 ff 02 01 1a 0a 01 00 30 81 ba 05 00 30 00 30 49 30 23 30 21 02 01 0a 30 1c 30 0e 30 0c 02 02 00 94 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 c0 0a 01 03 30 22 30 30 1f 30 08 02 01 00 30 03 02 01 00 30 13 02 01 01 30 0e 30 0c 30 30 03 02 01 0b 02 01 0f 02 01 00 30 69 30 67 30 65 02 01 0a 30 60 30 16 30 11 0a 01 00 0a 01 00 02 01 01 0a 01 04 05 00 02 01 01 02 01 01 30 16 30 11 0a 01 00 0a 01 00 02 01 02 0a 01 04 05 00 02 01 02 02 01 02 30 16 30 11 0a 01 00 0a 01 00 02 01 03 0a 01 04 05 00 02 01 03 02 01 03 30 16 30 11 0a 01 00 0a 01 00 02 01 04 0a 01 04 05 00 02 01 04 02 01 04

- No.: 254
- Timestamp: 10:52:01:633_0
- RFN: 156
- Chip: 26368
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_SS_1DCH_DCCH_Cfg LINE 9
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 1a

- No.: 255
- Timestamp: 10:52:01:639_0
- RFN: 157
- Chip: 11264
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_1DCH_DCCH_Cfg LINE 10
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
. (RatType)ratType = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . DPCHInfo
. . . . UL_DPCH_Info
. . . . . UL_DPCH_PowerControlInfo
. . . . . . fdd
. . . . . . . (IntegerType)dpcch_PowerOffset = -40
. . . . . . . (IntegerType)pc_Preamble = 1
. . . . . . . (IntegerType)sRB_delay = 7
. . . . . . . PowerControlAlgorithm
. . . . . . . . (IntegerType)algorithm1 = 1
. . . . . modeSpecificInfo
. . . . . . fdd
. . . . . . . (ScramblingCodeType)scramblingCodeType = 1
. . . . . . . (IntegerType)scramblingCode = 0
. . . . . . . (IntegerType)numberOfDPDCH = -
. . . . . . . (SpreadingFactor)spreadingFactor = 4
. . . . . . . (BooleanType)tfci_Existence = TRUE
. . . . . . . (IntegerType)numberOfFBI_Bits = -
. . . . . . . (PuncturingLimit)puncturingLimit = 15
. . . . DL_DPCHInfo
- Constraint:
ca_UL_DPCH_Info
- BinaryMessage:
30 30 02 01 00 02 01 14 0a 01 00 30 25 30 23 30 21 30 30 0c 02 01 d8 02 01 01 02 01 07 02 01 01 30 30 0f 0a 01 01 02 01 00 0a 01 04 01 01 ff 0a 01 0f

- No.: 259
- Timestamp: 10:52:01:645_0
- RFN: 157
- Chip: 36864
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_1DCH_DCCH_Cfg LINE 11
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 260
- Timestamp: 10:52:01:655_0
- RFN: 158
- Chip: 35584
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Config_REQ
- Source: ts_SS_1DCH_DCCH_Cfg LINE 12
- Message Structure:
CPHY_TrCH_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
. (RatType)ratType = 0
. CphyTrchConfigReq
. . SS_ActivationTime
. . ulconnectedTrCHList
. . . CphyTrchConfigReq_setseq_0
. . . . (IntegerType)trchid = 5
. . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 148
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional = 1
. . . . . . (IntegerType)rateMatchingAttribute = 192
. . . . . . (CRC_Size)crc_Size = 3
. . TFCS
. . . ExplicitTFCS_Configuration
. . . . TFCS_ReconfAdd
. . . . . ctfcSize
. . . . . . ctfc2Bit
. . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . (IntegerType)ctfc2 = 0
. . . . . . . . PowerOffsetInformation
. . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . (IntegerType)ctfc2 = 1
. . . . . . . . PowerOffsetInformation
. . dlconnectedTrCHList
. . TFCS
- Constraint:
ca_DCH_148_TTI_10_UL_InfoActNow
- BinaryMessage:
30 44 02 01 00 02 01 14 0a 01 00 30 39 05 00 30 26 30 24 02 01 05 0a 01 00 30 1c 30 0e 30 0c 02 02 00 94 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 c0 0a 01 03 30 0d 30 30 0a 30 03 02 01 00 30 03 02 01 01

- No.: 264
- Timestamp: 10:52:01:665_0
- RFN: 159
- Chip: 36864
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Config_CNF
- Source: ts_SS_1DCH_DCCH_Cfg LINE 13
- Message Structure:
CPHY_TrCH_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_TrChCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 265
- Timestamp: 10:52:01:699_0
- RFN: 163
- Chip: 13312
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_SS_1DCH_DCCH_Cfg LINE 14
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
. (RatType)ratType = 0
. configMessage
. . CmacConfigReq
. . . SS_ActivationTime
. . . UE_Info
. . . . U_RNTI
. . . . (BitStringType)c_RNTI[16] = -
. . . TrCHInfo
. . . . ulconnectedTrCHList
. . . . . TrCHInfo_setseq_0
. . . . . . (IntegerType)trchid = 5
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 148
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . (IntegerType)rateMatchingAttribute = 192
. . . . . . . . (CRC_Size)crc_Size = 3
. . . . TFCS
. . . . . ExplicitTFCS_Configuration
. . . . . . TFCS_ReconfAdd
. . . . . . . ctfcSize
. . . . . . . . ctfc2Bit
. . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . (IntegerType)ctfc2 = 0
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . (IntegerType)ctfc2 = 1
. . . . . . . . . . PowerOffsetInformation
. . . . dlconnectedTrCHList
. . . . TFCS
. . . TrCH_LogCHMappingList1
. . . . ulconnectedTrCHList
. . . . . TrCH_LogCHMappingList1_setseq_0
. . . . . . (IntegerType)trchid = 5
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . (IntegerType)rB_Identity = 1
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . (IntegerType)rB_Identity = 2
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . (IntegerType)rB_Identity = 3
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . (IntegerType)rB_Identity = 4
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . dlconnectedTrCHList
- Constraint:
ca_CMAC_CfgInfo
- BinaryMessage:
30 81 9d 02 01 ff 02 01 14 0a 01 00 30 81 91 05 00 30 00 30 34 30 23 30 21 02 01 05 30 1c 30 0e 30 0c 02 02 00 94 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 c0 0a 01 03 30 0d 30 30 0a 30 03 02 01 00 30 03 02 01 01 30 55 30 53 30 51 02 01 05 30 4c 30 11 30 0c 0a 01 00 0a 01 00 02 01 01 0a 01 04 02 01 01 30 11 30 0c 0a 01 00 0a 01 00 02 01 02 0a 01 04 02 01 02 30 11 30 0c 0a 01 00 0a 01 00 02 01 03 0a 01 04 02 01 03 30 11 30 0c 0a 01 00 0a 01 00 02 01 04 0a 01 04 02 01 04

- No.: 269
- Timestamp: 10:52:01:718_0
- RFN: 165
- Chip: 11264
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_SS_1DCH_DCCH_Cfg LINE 15
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 14

- No.: 272
- Timestamp: 10:52:01:724_0
- RFN: 165
- Chip: 33792
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB_BCCH_BCH_Cfg LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 246
. . . . . UL_RLC_Mode
. . . . . . UL_TM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . (BooleanType)segmentationIndication = FALSE
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = -
. . . . (IntegerType)dLlogicalChannelIdentity = 1
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_BCCH_Info
- BinaryMessage:
30 1d 02 01 00 02 01 ff 0a 01 00 30 12 30 0b 30 09 02 02 00 f6 30 03 01 01 00 30 03 02 01 01

- No.: 276
- Timestamp: 10:52:01:732_0
- RFN: 166
- Chip: 27136
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB_BCCH_BCH_Cfg LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 279
- Timestamp: 10:52:01:738_0
- RFN: 167
- Chip: 11008
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB_PCCH_Cfg LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -2
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 240
. . . . . UL_RLC_Mode
. . . . . . UL_TM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . (BooleanType)segmentationIndication = FALSE
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = -
. . . . (IntegerType)dLlogicalChannelIdentity = 1
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_PCCH_Info
- BinaryMessage:
30 1d 02 01 00 02 01 fe 0a 01 00 30 12 30 0b 30 09 02 02 00 f0 30 03 01 01 00 30 03 02 01 01

- No.: 283
- Timestamp: 10:52:01:743_0
- RFN: 167
- Chip: 30208
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB_PCCH_Cfg LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 fe

- No.: 286
- Timestamp: 10:52:01:749_0
- RFN: 168
- Chip: 14336
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB0_Cfg LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 152
. . . . . UL_RLC_Mode
. . . . . . UL_UM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (NoExplicitDiscard)timerBasedNoExplicit = 9
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = -
. . . . (IntegerType)dLlogicalChannelIdentity = 5
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_UM_DL_Info
- BinaryMessage:
30 1d 02 01 00 02 01 00 0a 01 00 30 12 30 0b 30 09 02 02 00 98 30 03 0a 01 09 30 03 02 01 05

- No.: 290
- Timestamp: 10:52:01:756_0
- RFN: 169
- Chip: 4608
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB0_Cfg LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 00

- No.: 291
- Timestamp: 10:52:01:763_0
- RFN: 169
- Chip: 28672
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB0_Cfg LINE 3
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_TM_RLC_Mode
. . . . . . (BooleanType)segmentationIndication = TRUE
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 166
. . . . . UL_RLC_Mode
. . . . . . UL_TM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . (BooleanType)segmentationIndication = TRUE
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = 5
. . . . (IntegerType)dLlogicalChannelIdentity = -
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_TM_UL_Info
- BinaryMessage:
30 22 02 01 00 02 01 00 0a 01 00 30 17 30 10 30 03 01 01 ff 30 09 02 02 00 a6 30 03 01 01 ff 30 03 02 01 05

- No.: 295
- Timestamp: 10:52:01:773_0
- RFN: 170
- Chip: 29184
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB0_Cfg LINE 4
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 00

- No.: 298
- Timestamp: 10:52:01:781_0
- RFN: 171
- Chip: 19712
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 136
. . . . . UL_RLC_Mode
. . . . . . UL_UM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (NoExplicitDiscard)timerBasedNoExplicit = 9
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = 1
. . . . (IntegerType)dLlogicalChannelIdentity = 1
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_UM_Info
- BinaryMessage:
30 22 02 01 ff 02 01 01 0a 01 00 30 17 30 0d 05 00 30 09 02 02 00 88 30 03 0a 01 09 30 06 02 01 01 02 01 01

- No.: 302
- Timestamp: 10:52:01:789_0
- RFN: 172
- Chip: 9472
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 303
- Timestamp: 10:52:01:798_0
- RFN: 173
- Chip: 5632
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 3
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . (TimerEPC)timerEPC = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . (TimerRST)timerRST = 9
. . . . . . . (MaxRST)max_RST = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = 2
. . . . (IntegerType)dLlogicalChannelIdentity = 2
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 02 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 27 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 02 02 01 02

- No.: 307
- Timestamp: 10:52:01:817_0
- RFN: 175
- Chip: 3840
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 4
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 308
- Timestamp: 10:52:01:826_0
- RFN: 175
- Chip: 38144
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 5
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . (TimerEPC)timerEPC = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . (TimerRST)timerRST = 9
. . . . . . . (MaxRST)max_RST = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = 3
. . . . (IntegerType)dLlogicalChannelIdentity = 3
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 03 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 27 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 03 02 01 03

- No.: 312
- Timestamp: 10:52:01:847_0
- RFN: 178
- Chip: 2560
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 6
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 313
- Timestamp: 10:52:01:856_0
- RFN: 178
- Chip: 37376
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 7
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . (TimerEPC)timerEPC = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . (TimerRST)timerRST = 9
. . . . . . . (MaxRST)max_RST = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = 4
. . . . (IntegerType)dLlogicalChannelIdentity = 4
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 04 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 27 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 04 02 01 04

- No.: 317
- Timestamp: 10:52:01:877_0
- RFN: 181
- Chip: 3584
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 8
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 358
- Timestamp: 10:52:01:923_0
- RFN: 185
- Chip: 27136
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 27
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 1b

- No.: 363
- Timestamp: 10:52:01:928_0
- RFN: 186
- Chip: 7424
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendNoSegDefSchedul LINE 2
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 364
- Timestamp: 10:52:01:931_0
- RFN: 186
- Chip: 21504
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendNoSegDefSchedul LINE 3
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 08 02 01 00 02 01 ff 00 00

- No.: 372
- Timestamp: 10:52:01:943_0
- RFN: 187
- Chip: 27904
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 11
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 0b

- No.: 377
- Timestamp: 10:52:01:948_0
- RFN: 188
- Chip: 7680
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB1 LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 378
- Timestamp: 10:52:01:953_0
- RFN: 188
- Chip: 28928
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB1 LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 1
. . . . . . . (BitStringType)sib_Data_variable[-1] = "1100010000000000000001011000100000101000000010100001000111100000000101000000000000000000000011000111010000"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 2
. . . . . . . (BitStringType)sib_Data_variable[-1] = "10000000000000000001"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 1c 02 01 00 02 01 ff 00 0e 21 69 c4 00 05 88 28 0a 11 e0 14 00 00 0c 74 04 27 00 00 20

- No.: 391
- Timestamp: 10:52:01:963_0
- RFN: 189
- Chip: 28416
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 11
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 0b

- No.: 396
- Timestamp: 10:52:01:968_0
- RFN: 190
- Chip: 8192
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB2 LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 397
- Timestamp: 10:52:01:973_0
- RFN: 190
- Chip: 29696
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB2 LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 1
. . . . . . . (BitStringType)sib_Data_variable[-1] = "1100010000000000000001011000100000101000000010100001000111100000000101000000000000000000000011000111010000"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 2
. . . . . . . (BitStringType)sib_Data_variable[-1] = "10000000000000000001"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 1c 02 01 00 02 01 ff 00 0e 21 69 c4 00 05 88 28 0a 11 e0 14 00 00 0c 74 04 27 00 00 20

- No.: 409
- Timestamp: 10:52:01:983_0
- RFN: 191
- Chip: 28928
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 10
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 0a

- No.: 414
- Timestamp: 10:52:01:988_0
- RFN: 192
- Chip: 8448
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB3 LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 415
- Timestamp: 10:52:01:993_0
- RFN: 192
- Chip: 28160
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB3 LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 7
. . . . . . . (BitStringType)sib_Data_variable[-1] = "101000101000000010000001"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 3
. . . . . . . (BitStringType)sib_Data_variable[-1] = "110000000000000000000000000000000100000011001100011000000000100100001000000100011111111111111111111111"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 1c 02 01 00 02 01 ff 00 0e 27 17 a2 80 81 1b 2e 00 00 00 02 06 63 00 48 40 8f ff ff e0

- No.: 427
- Timestamp: 10:52:02:004_0
- RFN: 193
- Chip: 30720
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 26
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 1a

- No.: 432
- Timestamp: 10:52:02:008_0
- RFN: 194
- Chip: 11264
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB4 LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 433
- Timestamp: 10:52:02:014_0
- RFN: 194
- Chip: 32768
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB4 LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 7
. . . . . . . (BitStringType)sib_Data_variable[-1] = "101000101000000010000001"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 4
. . . . . . . (BitStringType)sib_Data_variable[-1] = "1000000000000000000000000000000101100110001100000000010010000100000010001110111"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 19 02 01 00 02 01 ff 00 0e 27 17 a2 80 81 22 74 00 00 00 0b 31 80 24 20 47 70

- No.: 450
- Timestamp: 10:52:02:060_0
- RFN: 199
- Chip: 17152
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 23
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 17

- No.: 455
- Timestamp: 10:52:02:064_0
- RFN: 199
- Chip: 34816
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB5 LINE 41
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 456
- Timestamp: 10:52:02:068_0
- RFN: 200
- Chip: 11520
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB5 LINE 42
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 08 02 01 00 02 01 ff 00 00

- No.: 460
- Timestamp: 10:52:02:072_0
- RFN: 200
- Chip: 26880
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 19
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 13

- No.: 465
- Timestamp: 10:52:02:084_0
- RFN: 201
- Chip: 35072
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB5 LINE 44
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 466
- Timestamp: 10:52:02:089_0
- RFN: 202
- Chip: 14080
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB5 LINE 45
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . FirstSegment
. . . . . . (SIB_Type)sib_Type = 5
. . . . . . (IntegerType)seg_Count = 3
. . . . . . (BitStringType)sib_Data_fixed[222] = "001101010100010000111110000000001111111101000011111111111111110111010010000100001111000000101001000011000000101010100101010110000000000000001100110001011011010101111110001010111010000011111110100000111111101000001111111010"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 25 02 01 00 02 01 ff 00 02 52 35 44 3e 00 ff 43 ff fd d2 10 f0 29 0c 0a a5 58 00 0c c5 b5 7e 2b a0 fe 83 fa 0f e8

- No.: 470
- Timestamp: 10:52:02:095_0
- RFN: 202
- Chip: 31488
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 21
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 15

- No.: 475
- Timestamp: 10:52:02:105_0
- RFN: 203
- Chip: 34816
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB5 LINE 47
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 476
- Timestamp: 10:52:02:110_0
- RFN: 204
- Chip: 15104
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB5 LINE 48
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . SubsequentSegment
. . . . . . (SIB_Type)sib_Type = 5
. . . . . . (IntegerType)segmentIndex = 1
. . . . . . (BitStringType)sib_Data_fixed[222] = "000011111111010000000000000000001101011000110100010000111111010011100101000001100001000011001010000000110000001110001001000000010110000000000000100000001110000000001000100001100100001010011001000010100000000000110000000100"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 25 02 01 00 02 01 ff 00 04 50 0f f4 00 00 d6 34 43 f4 e5 06 10 ca 03 03 89 01 60 00 80 e0 08 86 42 99 0a 00 30 10

- No.: 480
- Timestamp: 10:52:02:115_0
- RFN: 204
- Chip: 32000
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 22
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 16

- No.: 485
- Timestamp: 10:52:02:125_0
- RFN: 205
- Chip: 34560
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB5 LINE 50
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 487
- Timestamp: 10:52:02:130_0
- RFN: 206
- Chip: 15360
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB5 LINE 52
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . LastSegmentShort
. . . . . . (SIB_Type)sib_Type = 5
. . . . . . (IntegerType)segmentIndex = 2
. . . . . . (BitStringType)sib_Data_variable[-1] = "010001011100101011010110100000000000011110001000011000000001011011011011011000100000000001000011000010001001010000001011011010000000010000"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 1c 02 01 00 02 01 ff 00 06 51 89 45 ca d6 80 07 88 60 16 db 62 00 43 08 94 0b 68 04 00

- No.: 504
- Timestamp: 10:52:02:145_0
- RFN: 207
- Chip: 35584
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 3
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 03

- No.: 509
- Timestamp: 10:52:02:154_0
- RFN: 208
- Chip: 31232
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB6 LINE 8
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 512
- Timestamp: 10:52:02:159_0
- RFN: 209
- Chip: 11520
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB6:lt_CompleteSIB LINE 4
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 6
. . . . . . . (BitStringType)sib_Data_variable[-1] = "0000001010010001"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 0c 02 01 00 02 01 ff 00 0e 06 0f 02 91

- No.: 517
- Timestamp: 10:52:02:164_0
- RFN: 209
- Chip: 29440
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 5
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 05

- No.: 522
- Timestamp: 10:52:02:175_0
- RFN: 210
- Chip: 33280
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB6 LINE 11
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 523
- Timestamp: 10:52:02:179_0
- RFN: 211
- Chip: 10240
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB6 LINE 12
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 08 02 01 00 02 01 ff 00 00

- No.: 527
- Timestamp: 10:52:02:183_0
- RFN: 211
- Chip: 25600
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 6
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 06

- No.: 532
- Timestamp: 10:52:02:195_0
- RFN: 212
- Chip: 33792
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB6 LINE 14
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 533
- Timestamp: 10:52:02:199_0
- RFN: 213
- Chip: 10496
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB6 LINE 15
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 08 02 01 00 02 01 ff 00 00

- No.: 537
- Timestamp: 10:52:02:203_0
- RFN: 213
- Chip: 25344
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 7
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 07

- No.: 542
- Timestamp: 10:52:02:215_0
- RFN: 214
- Chip: 34304
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB6 LINE 17
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 543
- Timestamp: 10:52:02:219_0
- RFN: 215
- Chip: 11008
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB6 LINE 18
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 08 02 01 00 02 01 ff 00 00

- No.: 551
- Timestamp: 10:52:02:233_0
- RFN: 216
- Chip: 25600
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 2
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 02

- No.: 556
- Timestamp: 10:52:02:240_0
- RFN: 217
- Chip: 16128
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB7 LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 559
- Timestamp: 10:52:02:248_0
- RFN: 218
- Chip: 7680
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB7:lt_CompleteSIB LINE 4
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 7
. . . . . . . (BitStringType)sib_Data_variable[-1] = "101000101000000010000001"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 0d 02 01 00 02 01 ff 00 0e 07 17 a2 80 81

- No.: 567
- Timestamp: 10:52:02:263_0
- RFN: 219
- Chip: 28928
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 10
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 0a

- No.: 572
- Timestamp: 10:52:02:271_0
- RFN: 220
- Chip: 18688
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB7:lt_ConcatWithSIB3 LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 573
- Timestamp: 10:52:02:277_0
- RFN: 221
- Chip: 5632
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB7:lt_ConcatWithSIB3 LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 7
. . . . . . . (BitStringType)sib_Data_variable[-1] = "101000101000000010000001"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 3
. . . . . . . (BitStringType)sib_Data_variable[-1] = "110000000000000000000000000000000100000011001100011000000000100100001000000100011111111111111111111111"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 1c 02 01 00 02 01 ff 00 0e 27 17 a2 80 81 1b 2e 00 00 00 02 06 63 00 48 40 8f ff ff e0

- No.: 581
- Timestamp: 10:52:02:291_0
- RFN: 222
- Chip: 22016
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 18
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 12

- No.: 586
- Timestamp: 10:52:02:299_0
- RFN: 223
- Chip: 12288
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB7:lt_ConcatWithSIB18 LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 587
- Timestamp: 10:52:02:305_0
- RFN: 223
- Chip: 36352
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB7:lt_ConcatWithSIB18 LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 7
. . . . . . . (BitStringType)sib_Data_variable[-1] = "101000101000000010000001"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 26
. . . . . . . (BitStringType)sib_Data_variable[-1] = "100100000001000000000001000000001"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 13 02 01 00 02 01 ff 00 0e 27 17 a2 80 81 d1 04 80 80 08 04

- No.: 595
- Timestamp: 10:52:02:319_0
- RFN: 225
- Chip: 14336
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 26
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 1a

- No.: 600
- Timestamp: 10:52:02:327_0
- RFN: 226
- Chip: 5632
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB7:lt_ConcatWithSIB4 LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 601
- Timestamp: 10:52:02:334_0
- RFN: 226
- Chip: 30720
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB7:lt_ConcatWithSIB4 LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 7
. . . . . . . (BitStringType)sib_Data_variable[-1] = "101000101000000010000001"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 4
. . . . . . . (BitStringType)sib_Data_variable[-1] = "1000000000000000000000000000000101100110001100000000010010000100000010001110111"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 19 02 01 00 02 01 ff 00 0e 27 17 a2 80 81 22 74 00 00 00 0b 31 80 24 20 47 70

- No.: 615
- Timestamp: 10:52:02:345_0
- RFN: 227
- Chip: 35072
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 31
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 1f

- No.: 620
- Timestamp: 10:52:02:354_0
- RFN: 228
- Chip: 32256
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB11 LINE 20
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 621
- Timestamp: 10:52:02:358_0
- RFN: 229
- Chip: 8960
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB11 LINE 21
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 08 02 01 00 02 01 ff 00 00

- No.: 625
- Timestamp: 10:52:02:362_0
- RFN: 229
- Chip: 24576
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 29
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 1d

- No.: 630
- Timestamp: 10:52:02:374_0
- RFN: 230
- Chip: 34048
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB11 LINE 23
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 631
- Timestamp: 10:52:02:379_0
- RFN: 231
- Chip: 14336
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB11 LINE 24
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . FirstSegment
. . . . . . (SIB_Type)sib_Type = 11
. . . . . . (IntegerType)seg_Count = 2
. . . . . . (BitStringType)sib_Data_fixed[222] = "011000001101100100010010000000001000110010000100001000010010010110101000100000100110010001010011000001011001000010100111000010111000010100001000100010001100100101010100000001001010000101001010100001100001001010001000001010"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 25 02 01 00 02 01 ff 00 02 b1 60 d9 12 00 8c 84 21 25 a8 82 64 53 05 90 a7 0b 85 08 88 c9 54 04 a1 4a 86 12 88 28

- No.: 635
- Timestamp: 10:52:02:384_0
- RFN: 231
- Chip: 32000
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 30
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 1e

- No.: 640
- Timestamp: 10:52:02:394_0
- RFN: 232
- Chip: 33792
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB11 LINE 26
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 642
- Timestamp: 10:52:02:399_0
- RFN: 233
- Chip: 14848
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB11 LINE 28
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . LastSegmentShort
. . . . . . (SIB_Type)sib_Type = 11
. . . . . . (IntegerType)segmentIndex = 1
. . . . . . (BitStringType)sib_Data_variable[-1] = "000100001100001001010010011010101000011000010010101000101100011001010100101010100001001111101000100010000001010010110000100010100001010101111000"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 1c 02 01 00 02 01 ff 00 06 b0 8f 10 c2 52 6a 86 12 a2 c6 54 aa 13 e8 88 14 b0 8a 15 78

- No.: 655
- Timestamp: 10:52:02:409_0
- RFN: 234
- Chip: 11776
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 13
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 0d

- No.: 660
- Timestamp: 10:52:02:416_0
- RFN: 234
- Chip: 37376
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB12 LINE 8
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 663
- Timestamp: 10:52:02:421_0
- RFN: 235
- Chip: 19968
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB12:lt_CompleteSIB LINE 4
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 12
. . . . . . . (BitStringType)sib_Data_variable[-1] = "010000000"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 0c 02 01 00 02 01 ff 00 0e 0c 08 40 00

- No.: 668
- Timestamp: 10:52:02:426_0
- RFN: 235
- Chip: 36352
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 14
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 0e

- No.: 673
- Timestamp: 10:52:02:435_0
- RFN: 236
- Chip: 32512
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB12 LINE 11
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 674
- Timestamp: 10:52:02:438_0
- RFN: 237
- Chip: 8192
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB12 LINE 12
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 08 02 01 00 02 01 ff 00 00

- No.: 678
- Timestamp: 10:52:02:443_0
- RFN: 237
- Chip: 24832
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 15
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 0f

- No.: 683
- Timestamp: 10:52:02:455_0
- RFN: 238
- Chip: 33280
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB12 LINE 14
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 684
- Timestamp: 10:52:02:459_0
- RFN: 239
- Chip: 9984
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB12 LINE 15
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 08 02 01 00 02 01 ff 00 00

- No.: 692
- Timestamp: 10:52:02:467_0
- RFN: 240
- Chip: 3072
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 18
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 12

- No.: 697
- Timestamp: 10:52:02:476_0
- RFN: 240
- Chip: 37888
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB18 LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 698
- Timestamp: 10:52:02:481_0
- RFN: 241
- Chip: 19712
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB18 LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 7
. . . . . . . (BitStringType)sib_Data_variable[-1] = "101000101000000010000001"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 26
. . . . . . . (BitStringType)sib_Data_variable[-1] = "100100000001000000000001000000001"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 13 02 01 00 02 01 ff 00 0e 27 17 a2 80 81 d1 04 80 80 08 04

- No.: 710
- Timestamp: 10:52:02:490_0
- RFN: 242
- Chip: 14336
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 4
. . (IntegerType)sg_POS = 1
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 04 02 01 01

- No.: 715
- Timestamp: 10:52:02:496_0
- RFN: 242
- Chip: 37632
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSB1_DefSchedul LINE 4
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 718
- Timestamp: 10:52:02:501_0
- RFN: 243
- Chip: 19712
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSB1_DefSchedul:lt_CompleteSIB LINE 4
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 27
. . . . . . . (BitStringType)sib_Data_variable[-1] = "10010000101010001000001100110000010010010100111000101001110100000000010110100010001101110010100010010010"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 17 02 01 00 02 01 ff 00 0e 1b 67 90 a8 83 30 49 4e 29 d0 05 a2 37 28 92

- No.: 736
- Timestamp: 10:52:02:513_0
- RFN: 244
- Chip: 25856
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 3
. . (IntegerType)sg_POS = 0
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 03 02 01 00

- No.: 741
- Timestamp: 10:52:02:517_0
- RFN: 245
- Chip: 4864
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendMIB LINE 7
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 744
- Timestamp: 10:52:02:523_0
- RFN: 245
- Chip: 26624
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendMIB:lt_CompleteSIB LINE 4
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 0
. . . . . . . (BitStringType)sib_Data_variable[-1] = "0001000000000000010000000010010110101010000100010000000000001000100010110000101000100010110001001000100010100001101000100110100010001110010010010011000100010000"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 1e 02 01 00 02 01 ff 00 0e 00 9f 10 00 40 25 aa 11 00 08 8b 0a 22 c4 88 a1 a2 68 8e 49 31 10

- No.: 759
- Timestamp: 10:52:02:529_0
- RFN: 246
- Chip: 13568
- Event: Send
- PCO: Ut
- Message: MMI_CmdReq
- Source: ts_MMI_UE_SwitchOn LINE 1
- Message Structure:
MMI_CmdReq
. (IA5StringType)cmd[-1] = "Please switch on the UE"
- Constraint:
ca_MMI_CmdReq
- BinaryMessage:
50 6c 65 61 73 65 20 73 77 69 74 63 68 20 6f 6e 20 74 68 65 20 55 45

- No.: 763
- Timestamp: 10:52:10:870_0
- RFN: 1080
- Chip: 16384
- Event: Receive
- PCO: Ut
- Message: MMI_CmdCnf
- Source: ts_MMI_UE_SwitchOn LINE 2
- Message Structure:
MMI_CmdCnf
. (BooleanType)result = TRUE
. (IA5StringType)resultString[6] = " OK "
- Constraint:
ca_MMI_CmdCnf
- BinaryMessage:
80 0d 0a 4f 4b 0d 0a

- No.: 782
- Timestamp: 10:52:12:669_0
- RFN: 1260
- Chip: 13824
- Event: Receive
- PCO: TM
- Message: RLC_TR_DATA_IND
- Source: ts_RRC_ConnEst:lt_RcvConnReq LINE 2
- Message Structure:
RLC_TR_DATA_IND
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
. tM_message
. . UL_CCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode = 0
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . UL_CCCH_MessageType
. . . . RRCConnectionRequest
. . . . . InitialUE_Identity
. . . . . . TMSI_and_LAI_GSM_MAP
. . . . . . . (BitStringType)tmsi[32] = "00010010001101000101011001111000"
. . . . . . . LAI
. . . . . . . . PLMN_Identity
. . . . . . . . . MCC
. . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . (IntegerType)_elem = 1
. . . . . . . . . MNC
. . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . (IntegerType)_elem = 1
. . . . . . . . (BitStringType)lac[16] = '0000000000000001'B
. . . . . (EstablishmentCause)establishmentCause = 12
. . . . . (ProtocolErrorIndicator)protocolErrorIndicator = 0
. . . . . MeasuredResultsOnRACH
. . . . . . currentCell
. . . . . . . modeSpecificInfo
. . . . . . . . fdd
. . . . . . . . . measurementQuantity
. . . . . . . . . . (IntegerType)cpich_Ec_N0 = 0
. . . . . v3d0NonCriticalExtensions
. . . . . . RRCConnectionRequest_v3d0ext_IEs
. . . . . . . (BitStringType)uESpecificBehaviourInformation1idle = 0
. . . . . . nonCriticalExtensions
- Constraint:
car_RRC_ConnReq
- BinaryMessage:
30 11 02 01 00 02 01 00 21 12 34 56 78 00 10 08 00 0b 00

- No.: 786
- Timestamp: 10:52:12:731_0
- RFN: 1266
- Chip: 20992
- Event: Send
- PCO: UM
- Message: RLC_UM_DATA_REQ
- Source: ts_RRC_ConnEst:lt_Send_ConnSetUp LINE 22
- Message Structure:
RLC_UM_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
. uM_message
. . DL_CCCH_Message
. . . IntegrityCheckInfo
. . . DL_CCCH_MessageType
. . . . RRCConnectionSetup
. . . . . r3
. . . . . . RRCConnectionSetup_r3_IEs
. . . . . . . InitialUE_Identity
. . . . . . . . TMSI_and_LAI_GSM_MAP
. . . . . . . . . (BitStringType)tmsi[32] = "00010010001101000101011001111000"
. . . . . . . . . LAI
. . . . . . . . . . PLMN_Identity
. . . . . . . . . . . MCC
. . . . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . . . (IntegerType)_elem = 1
. . . . . . . . . . . MNC
. . . . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . . . (IntegerType)_elem = 1
. . . . . . . . . . (BitStringType)lac[16] = '0000000000000001'B
. . . . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . . . (IntegerType)activationTime = -
. . . . . . . U_RNTI
. . . . . . . . (BitStringType)srnc_Identity[12] = "000000000001"
. . . . . . . . (BitStringType)s_RNTI[20] = "00000000000000000001"
. . . . . . . (BitStringType)new_c_RNTI[16] = -
. . . . . . . (RRC_StateIndicator)rrc_StateIndicator = 0
. . . . . . . (IntegerType)utran_DRX_CycleLengthCoeff = 9
. . . . . . . CapabilityUpdateRequirement
. . . . . . . . (BooleanType)ue_RadioCapabilityFDDUpdateRequirement = TRUE
. . . . . . . . (BooleanType)ue_RadioCapabilityTDDUpdateRequirement = FALSE
. . . . . . . . SystemSpecificCapUpdateReqList
. . . . . . . . . (SystemSpecificCapUpdateReq)_elem = 0
. . . . . . . SRB_InformationSetupList2
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_UM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 1
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 1
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . . . . . . . (TimerRST)timerRST = 9
. . . . . . . . . . . . . (MaxRST)max_RST = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 2
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 2
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . . . . . . . (TimerRST)timerRST = 9
. . . . . . . . . . . . . (MaxRST)max_RST = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 3
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 3
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . . . . . . . (TimerRST)timerRST = 9
. . . . . . . . . . . . . (MaxRST)max_RST = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 4
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 4
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . UL_CommonTransChInfo
. . . . . . . . TFC_Subset
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . TFCS
. . . . . . . . . . . ExplicitTFCS_Configuration
. . . . . . . . . . . . TFCS_ReconfAdd
. . . . . . . . . . . . . ctfcSize
. . . . . . . . . . . . . . ctfc2Bit
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . . . . . . . (IntegerType)ctfc2 = 0
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . . . . . . . (IntegerType)ctfc2 = 1
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 11
. . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . UL_AddReconfTransChInfoList
. . . . . . . . UL_AddReconfTransChInformation
. . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType = 0
. . . . . . . . . (IntegerType)transportChannelIdentity = 5
. . . . . . . . . TransportFormatSet
. . . . . . . . . . DedicatedTransChTFS
. . . . . . . . . . . tti
. . . . . . . . . . . . DedicatedDynamicTF_InfoList
. . . . . . . . . . . . . DedicatedDynamicTF_Info
. . . . . . . . . . . . . . rlc_Size
. . . . . . . . . . . . . . . BitModeRLC_SizeInfo
. . . . . . . . . . . . . . . . sizeType2
. . . . . . . . . . . . . . . . . (IntegerType)part1 = 2
. . . . . . . . . . . . . . . . . (IntegerType)part2 = -
. . . . . . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . LogicalChannelList
. . . . . . . . . . . SemistaticTF_Information
. . . . . . . . . . . . ChannelCodingType
. . . . . . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . . . . . (IntegerType)rateMatchingAttribute = 192
. . . . . . . . . . . . (CRC_Size)crc_Size = 3
. . . . . . . DL_CommonTransChInfo
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . dl_Parameters
. . . . . . . DL_AddReconfTransChInfoList
. . . . . . . . DL_AddReconfTransChInformation
. . . . . . . . . (DL_TrCH_Type)dl_TransportChannelType = 0
. . . . . . . . . (IntegerType)dl_transportChannelIdentity = 10
. . . . . . . . . tfs_SignallingMode
. . . . . . . . . . UL_TransportChannelIdentity
. . . . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType = 0
. . . . . . . . . . . (IntegerType)ul_TransportChannelIdentity = 5
. . . . . . . . . QualityTarget
. . . . . . . . . . (IntegerType)bler_QualityValue = -20
. . . . . . . . . TM_SignallingInfo
. . . . . . . FrequencyInfo
. . . . . . . (IntegerType)maxAllowedUL_TX_Power = -
. . . . . . . UL_ChannelRequirement
. . . . . . . . UL_DPCH_Info
. . . . . . . . . UL_DPCH_PowerControlInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (IntegerType)dpcch_PowerOffset = -40
. . . . . . . . . . . (IntegerType)pc_Preamble = 1
. . . . . . . . . . . (IntegerType)sRB_delay = 7
. . . . . . . . . . . PowerControlAlgorithm
. . . . . . . . . . . . (IntegerType)algorithm1 = 1
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (ScramblingCodeType)scramblingCodeType = 1
. . . . . . . . . . . (IntegerType)scramblingCode = 0
. . . . . . . . . . . (IntegerType)numberOfDPDCH = -
. . . . . . . . . . . (SpreadingFactor)spreadingFactor = 4
. . . . . . . . . . . (BooleanType)tfci_Existence = TRUE
. . . . . . . . . . . (IntegerType)numberOfFBI_Bits = -
. . . . . . . . . . . (PuncturingLimit)puncturingLimit = 15
. . . . . . . DL_CommonInformation
. . . . . . . . DL_DPCH_InfoCommon
. . . . . . . . . cfnHandling
. . . . . . . . . . initialise
. . . . . . . . . . . (IntegerType)cfntargetsfnframeoffset = -
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . DL_DPCH_PowerControlInfo
. . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . (DPC_Mode)dpc_Mode = 0
. . . . . . . . . . . (IntegerType)powerOffsetPilot_pdpdch = 0
. . . . . . . . . . . Dl_rate_matching_restriction
. . . . . . . . . . . SF512_AndPilot
. . . . . . . . . . . . (PilotBits128)sfd128 = 0
. . . . . . . . . . . (PositionFixedOrFlexible)positionFixedOrFlexible = 0
. . . . . . . . . . . (BooleanType)tfci_Existence = FALSE
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . (IntegerType)defaultDPCH_OffsetValue = 0
. . . . . . . . . . DPCH_CompressedModeInfo
. . . . . . . . . . (TX_DiversityMode)tx_DiversityMode = 0
. . . . . . . . . . SSDT_Information
. . . . . . . DL_InformationPerRL_List
. . . . . . . . DL_InformationPerRL
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . PrimaryCPICH_Info
. . . . . . . . . . . . (IntegerType)primaryScramblingCode = 100
. . . . . . . . . . . PDSCH_SHO_DCH_Info
. . . . . . . . . . . PDSCH_CodeMapping
. . . . . . . . . DL_DPCH_InfoPerRL
. . . . . . . . . . fdd
. . . . . . . . . . . (PCPICH_UsageForChannelEst)pCPICH_UsageForChannelEst = 0
. . . . . . . . . . . (IntegerType)dpch_FrameOffset = 0
. . . . . . . . . . . SecondaryCPICH_Info
. . . . . . . . . . . DL_ChannelisationCodeList
. . . . . . . . . . . . DL_ChannelisationCode
. . . . . . . . . . . . . (IntegerType)secondaryScramblingCode = 1
. . . . . . . . . . . . . SF512_AndCodeNumber
. . . . . . . . . . . . . . (IntegerType)sf128 = 0
. . . . . . . . . . . . . (ScramblingCodeChange)scramblingCodeChange = 1
. . . . . . . . . . . (IntegerType)tpc_CombinationIndex = 0
. . . . . . . . . . . (SSDT_CellIdentity)ssdt_CellIdentity = -
. . . . . . . . . . . (ClosedLoopTimingAdjMode)closedLoopTimingAdjMode = -
. . . . . . . . . SCCPCH_InfoForFACH
. . . . . . laterNonCriticalExtensions
. (BooleanType)specialLI = TRUE
- Constraint:
cas_RRC_ConnSetup
- BinaryMessage:
30 78 02 01 00 02 01 00 30 e7 22 46 8a cf 00 02 01 00 01 00 04 00 00 4d 82 69 3a 10 10 89 0d 42 00 02 81 9e 8e 46 c9 ce 7c 9c 4e 74 20 a5 12 3a 8c 00 15 13 3d 1c 8d 93 9c f9 38 9c e8 42 52 24 b5 28 00 4a 46 7a 39 1b 27 39 f2 71 39 d0 86 b4 49 ea 70 00 d4 c8 00 06 25 2b f0 02 00 08 82 23 bf 66 08 98 95 a5 47 a2 00 00 01 3f 90 0a 14 00 02 06 40 00 0c 28 08 01 01 ff

- No.: 807
- Timestamp: 10:52:12:776_0
- RFN: 1270
- Chip: 35840
- Event: Start Timer
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 3
- Message Structure:
no details available
- Constraint:
t_WaitMS (13500 Ms)
- BinaryMessage:

- No.: 812
- Timestamp: 10:52:12:993_0
- RFN: 1292
- Chip: 30208
- Event: Receive
- PCO: CPHY
- Message: CPHY_Sync_IND
- Source: RRC_Def1 LINE 13
- Message Structure:
CPHY_Sync_IND
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_SyncInd
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 813
- Timestamp: 10:52:12:994_0
- RFN: 1292
- Chip: 32000
- Event: Cancel Timer
- Source: RRC_Def1 LINE 13
- Message Structure:
no details available
- Constraint:
t_T312
- BinaryMessage:

- No.: 814
- Timestamp: 10:52:12:995_0
- RFN: 1292
- Chip: 35072
- Event: Default
- Source: RRC_Def1 LINE 0
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 815
- Timestamp: 10:52:12:995_1
- RFN: 1292
- Chip: 35840
- Event: Default
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 820
- Timestamp: 10:52:13:189_0
- RFN: 1312
- Chip: 12032
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_IND
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
RLC_AM_DATA_IND
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. IntegrityResult
. . (IntegrityStatus)integrityUsed = 0
. aM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode = 0
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . UL_DCCH_MessageType
. . . . RRCConnectionSetupComplete
. . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . STARTList
. . . . . . STARTSingle
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity = 1
. . . . . . . (BitStringType)start_Value[20] = "00000000000000000100"
. . . . . . STARTSingle
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity = 0
. . . . . . . (BitStringType)start_Value[20] = "00000000000000000010"
. . . . . UE_RadioAccessCapability
. . . . . . (AccessStratumReleaseIndicator)accessStratumReleaseIndicator = 0
. . . . . . PDCP_Capability
. . . . . . . (BooleanType)losslessSRNS_RelocationSupport = FALSE
. . . . . . . supportForRfc2507
. . . . . . RLC_Capability
. . . . . . . (TotalRLC_AM_BufferSize)totalRLC_AM_BufferSize = 2
. . . . . . . (MaximumRLC_WindowSize)maximumRLC_WindowSize = 0
. . . . . . . (MaximumAM_EntityNumberRLC_Cap)maximumAM_EntityNumber = 3
. . . . . . TransportChannelCapability
. . . . . . . DL_TransChCapability
. . . . . . . . (MaxNoBits)maxNoBitsReceived = 4
. . . . . . . . (MaxNoBits)maxConvCodeBitsReceived = 1
. . . . . . . . TurboSupport
. . . . . . . . . (MaxNoBits)supported = 4
. . . . . . . . (MaxSimultaneousTransChsDL)maxSimultaneousTransChs = 1
. . . . . . . . (IntegerType)maxSimultaneousCCTrCH_Count = 1
. . . . . . . . (MaxTransportBlocksDL)maxReceivedTransportBlocks = 2
. . . . . . . . (MaxNumberOfTFC_DL)maxNumberOfTFC = 4
. . . . . . . . (MaxNumberOfTF)maxNumberOfTF = 1
. . . . . . . UL_TransChCapability
. . . . . . . . (MaxNoBits)maxNoBitsTransmitted = 3
. . . . . . . . (MaxNoBits)maxConvCodeBitsTransmitted = 1
. . . . . . . . TurboSupport
. . . . . . . . . (MaxNoBits)supported = 3
. . . . . . . . (MaxSimultaneousTransChsUL)maxSimultaneousTransChs = 2
. . . . . . . . modeSpecificInfo
. . . . . . . . (MaxTransportBlocksUL)maxTransmittedBlocks = 2
. . . . . . . . (MaxNumberOfTFC_UL)maxNumberOfTFC = 3
. . . . . . . . (MaxNumberOfTF)maxNumberOfTF = 0
. . . . . . RF_Capability
. . . . . . . fddRF_Capability
. . . . . . . . (IntegerType)ue_PowerClass = 4
. . . . . . . . (TxRxFrequencySeparation)txRxFrequencySeparation = 0
. . . . . . . tddRF_Capability
. . . . . . . . (IntegerType)ue_PowerClass = 0
. . . . . . . . (RadioFrequencyBandTDDList)radioFrequencyTDDBandList = 0
. . . . . . . . (ChipRateCapability)chipRateCapability = 0
. . . . . . PhysicalChannelCapability
. . . . . . . fddPhysChCapability
. . . . . . . . DL_PhysChCapabilityFDD
. . . . . . . . . (IntegerType)maxNoDPCH_PDSCH_Codes = 3
. . . . . . . . . (MaxNoPhysChBitsReceived)maxNoPhysChBitsReceived = 6
. . . . . . . . . (BooleanType)supportForSF_512 = FALSE
. . . . . . . . . (BooleanType)supportOfPDSCH = FALSE
. . . . . . . . . SimultaneousSCCPCH_DPCH_Reception
. . . . . . . . UL_PhysChCapabilityFDD
. . . . . . . . . (MaxNoDPDCH_BitsTransmitted)maxNoDPDCH_BitsTransmitted = 2
. . . . . . . . . (BooleanType)supportOfPCPCH = FALSE
. . . . . . . tddPhysChCapability
. . . . . . . . DL_PhysChCapabilityTDD
. . . . . . . . . (IntegerType)maxTS_PerFrame = 0
. . . . . . . . . (IntegerType)maxPhysChPerFrame = 0
. . . . . . . . . (MinimumSF_DL)minimumSF = 0
. . . . . . . . . (BooleanType)supportOfPDSCH = FALSE
. . . . . . . . . (IntegerType)maxPhysChPerTS = 0
. . . . . . . . UL_PhysChCapabilityTDD
. . . . . . . . . (IntegerType)maxTS_PerFrame = 0
. . . . . . . . . (MaxPhysChPerTimeslot)maxPhysChPerTimeslot = 0
. . . . . . . . . (MinimumSF_UL)minimumSF = 0
. . . . . . . . . (BooleanType)supportOfPUSCH = FALSE
. . . . . . UE_MultiModeRAT_Capability
. . . . . . . MultiRAT_Capability
. . . . . . . . (BooleanType)supportOfGSM = TRUE
. . . . . . . . (BooleanType)supportOfMulticarrier = FALSE
. . . . . . . (MultiModeCapability)multiModeCapability = 1
. . . . . . SecurityCapability
. . . . . . . (BitStringType)cipheringAlgorithmCap[16] = '0000000000000011'B
. . . . . . . (BitStringType)integrityProtectionAlgorithmCap[16] = '0000000000000010'B
. . . . . . UE_Positioning_Capability
. . . . . . . (BooleanType)standaloneLocMethodsSupported = FALSE
. . . . . . . (BooleanType)ue_BasedOTDOA_Supported = FALSE
. . . . . . . (NetworkAssistedGPS_Supported)networkAssistedGPS_Supported = 3
. . . . . . . (BooleanType)supportForUE_GPS_TimingOfCellFrames = FALSE
. . . . . . . (BooleanType)supportForIPDL = FALSE
. . . . . . MeasurementCapability
. . . . . . . CompressedModeMeasCapability
. . . . . . . . (BooleanType)fdd_Measurements = TRUE
. . . . . . . . (BooleanType)tdd_Measurements = FALSE
. . . . . . . . GSM_Measurements
. . . . . . . . . (BooleanType)gsm900 = TRUE
. . . . . . . . . (BooleanType)dcs1800 = TRUE
. . . . . . . . . (BooleanType)gsm1900 = FALSE
. . . . . . . . (BooleanType)multiCarrierMeasurements = FALSE
. . . . . . . CompressedModeMeasCapability
. . . . . . . . (BooleanType)fdd_Measurements = TRUE
. . . . . . . . (BooleanType)tdd_Measurements = FALSE
. . . . . . . . GSM_Measurements
. . . . . . . . . (BooleanType)gsm900 = TRUE
. . . . . . . . . (BooleanType)dcs1800 = TRUE
. . . . . . . . . (BooleanType)gsm1900 = FALSE
. . . . . . . . (BooleanType)multiCarrierMeasurements = FALSE
. . . . . v370NonCriticalExtensions
. . . . . . RRCConnectionSetupComplete_v370ext
. . . . . . . UE_RadioAccessCapability_v370ext
. . . . . . v380NonCriticalExtensions
. . . . . . . RRCConnectionSetupComplete_v380ext_IEs
. . . . . . . . UE_RadioAccessCapability_v380ext
. . . . . . . . . UE_PositioningCapabilityExt_v380
. . . . . . . . . . (BooleanType)rx_tx_TimeDifferenceType2Capable = FALSE
. . . . . . . . DL_PhysChCapabilityFDD_v380ext
. . . . . . . . . (SupportOfDedicatedPilotsForChEstimation)supportOfDedicatedPilotsForChEstimation = 0
. . . . . . . v3a0NonCriticalExtensions
. . . . . . . . RRCConnectionSetupComplete_v3a0ext_IEs
. . . . . . . . . UE_RadioAccessCapability_v3a0ext
. . . . . . . . . . UE_PositioningCapabilityExt_v3a0
. . . . . . . . . . . (UE_PositioningCapabilityExt_v3a0_list_0)validity_CellPCH_UraPCH = 0
. . . . . . . . laterNonCriticalExtensions
. . . . . . . . . (BitStringType)rrcConnectionSetupComplete_r3_add_ext = 0
. . . . . . . . . nonCriticalExtensions
- Constraint:
car_RRC_ConnSetupCmpl
- BinaryMessage:
30 27 02 01 ff 02 01 02 0a 05 01 00 00 00 00 4a 0c 00 01 00 00 05 11 a0 d1 04 84 c6 68 46 2c 93 02 48 00 18 00 11 8f 8f 80

- No.: 821
- Timestamp: 10:52:13:211_0
- RFN: 1314
- Chip: 18688
- Event: Cancel Timer
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
t_WaitMS
- BinaryMessage:

- No.: 822
- Timestamp: 10:52:13:211_1
- RFN: 1314
- Chip: 19456
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 836
- Timestamp: 10:52:13:228_0
- RFN: 1316
- Chip: 6912
- Event: Send
- PCO: CMAC
- Message: CMAC_SecurityMode_Config_REQ
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 1
- Message Structure:
CMAC_SecurityMode_Config_REQ
. (IntegerType)cellId = 0
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity = 1
. . (BitStringType)startValue[20] = "00000000000000000100"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = -
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CMAC_SecurityModeCfgReq
- BinaryMessage:
30 0e 02 01 00 30 09 0a 01 01 03 04 04 00 00 40

- No.: 837
- Timestamp: 10:52:13:229_0
- RFN: 1316
- Chip: 13568
- Event: Receive
- PCO: CMAC
- Message: CMAC_SecurityMode_Config_CNF
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 2
- Message Structure:
CMAC_SecurityMode_Config_CNF
. (IntegerType)cellId = 0
- Constraint:
ca_CMAC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 00

- No.: 838
- Timestamp: 10:52:13:239_0
- RFN: 1317
- Chip: 11264
- Event: Send
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_REQ
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 3
- Message Structure:
CRLC_SecurityMode_Config_REQ
. (IntegerType)cellId = -1
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity = 1
. . (BitStringType)startValue[20] = "00000000000000000100"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = -
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CRLC_SecurityModeCfgReq
- BinaryMessage:
30 0e 02 01 ff 30 09 0a 01 01 03 04 04 00 00 40

- No.: 839
- Timestamp: 10:52:13:241_0
- RFN: 1317
- Chip: 19712
- Event: Receive
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_CNF
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 4
- Message Structure:
CRLC_SecurityMode_Config_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 853
- Timestamp: 10:52:13:246_0
- RFN: 1318
- Chip: 1280
- Event: Send
- PCO: CMAC
- Message: CMAC_SecurityMode_Config_REQ
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 1
- Message Structure:
CMAC_SecurityMode_Config_REQ
. (IntegerType)cellId = 0
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity = 0
. . (BitStringType)startValue[20] = "00000000000000000010"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = -
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CMAC_SecurityModeCfgReq
- BinaryMessage:
30 0e 02 01 00 30 09 0a 01 00 03 04 04 00 00 20

- No.: 854
- Timestamp: 10:52:13:248_0
- RFN: 1318
- Chip: 7680
- Event: Receive
- PCO: CMAC
- Message: CMAC_SecurityMode_Config_CNF
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 2
- Message Structure:
CMAC_SecurityMode_Config_CNF
. (IntegerType)cellId = 0
- Constraint:
ca_CMAC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 00

- No.: 855
- Timestamp: 10:52:13:250_0
- RFN: 1318
- Chip: 15104
- Event: Send
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_REQ
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 3
- Message Structure:
CRLC_SecurityMode_Config_REQ
. (IntegerType)cellId = -1
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity = 0
. . (BitStringType)startValue[20] = "00000000000000000010"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = -
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CRLC_SecurityModeCfgReq
- BinaryMessage:
30 0e 02 01 ff 30 09 0a 01 00 03 04 04 00 00 20

- No.: 856
- Timestamp: 10:52:13:251_0
- RFN: 1318
- Chip: 21248
- Event: Receive
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_CNF
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 4
- Message Structure:
CRLC_SecurityMode_Config_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 863
- Timestamp: 10:52:13:332_0
- RFN: 1326
- Chip: 26112
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_GMM_IdleUpdated:lt_IdleUpdated_NMO_II LINE 3
- Message Structure:
RRC_DataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain = 0
. (START_Value)start[20] = '00000000000000000010'B
. LOCATIONUPDATINGREQUEST
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)mMProtocolDiscriminator[4] = '0101'B
. . (MsgType)msgType[8] = '00001000'B
. . CiphKeySeqNum
. . . (B1)spare1[1] = '0'B
. . . (KeySeq)keySeq[3] = '000'B
. . LocUpdType
. . . (B1)fOR[1] = '0'B
. . . (B1)spare1[1] = '0'B
. . . (B2)lUT[2] = '10'B
. . LocAreaId_v
. . . (OctetStringType)plmn[3] = '00F110'O
. . . (OctetStringType)lac[2] = '0001'O
. . MS_Clsmk1
. . . (B1)spare1[1] = '0'B
. . . (B2)revLvl[2] = '10'B
. . . (B1)eSIND[1] = '0'B
. . . (B1)a5_1[1] = '1'B
. . . (B3)rFPwrCap[3] = '111'B
. . MS_Identity_lv
. . . (Length)iel[1] = '05'O
. . . (B4)iDigit1[4] = '1111'B
. . . (B1)oddEvenInd[1] = '0'B
. . . (B3)typeOfId[3] = '100'B
. . . (OctetStringType)otherDigits[4] = '12345678'O
. . MS_Clsmk2
. . . (IEI8)iei[8] = '00110011'B
. . . (Length)iel[1] = '03'O
. . . (B1)spare1_1[1] = '0'B
. . . (B2)revLvl[2] = '10'B
. . . (B1)eSIND[1] = '0'B
. . . (B1)a5_1[1] = '1'B
. . . (B3)rFPwrCap[3] = '111'B
. . . (B1)spare1_2[1] = '0'B
. . . (B1)pSCap[1] = '0'B
. . . (B2)sSSI[2] = '01'B
. . . (B1)sMCap[1] = '1'B
. . . (B1)vBS[1] = '0'B
. . . (B1)vGCS[1] = '0'B
. . . (B1)fC[1] = '0'B
. . . (B1)cM3[1] = '1'B
. . . (B1)spare1_3[1] = '0'B
. . . (B1)lCSVA[1] = '0'B
. . . (B1)uCS2[1] = '0'B
. . . (B1)soLSA[1] = '0'B
. . . (B1)cMSP[1] = '0'B
. . . (B1)a5_3[1] = '0'B
. . . (B1)a5_2[1] = '0'B
- Constraint:
car_InitDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 00 03 04 04 00 00 20 05 08 02 00 f1 10 00 01 4f 05 f4 12 34 56 78 33 03 4f 18 80

- No.: 900
- Timestamp: 10:52:13:391_0
- RFN: 1332
- Chip: 16896
- Event: Send
- PCO: Dc
- Message: RRC_DataReq
- Source: ts_MM_Authentication LINE 2
- Message Structure:
RRC_DataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[-1] = -
. (SapId)sapId[1] = -
. (SS_CN_DomainIdentity)cN_Domain = 0
. AUTHENTICATIONREQUEST
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)mMProtocolDiscriminator[4] = '0101'B
. . (MsgType)msgType[8] = '00010010'B
. . (B4)spare4[4] = '0000'B
. . CiphKeySeqNum
. . . (B1)spare1[1] = '0'B
. . . (KeySeq)keySeq[3] = '000'B
. . (MM_RAND)rAND[128] = '01010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101'B
. . AUTN
. . . (IEI8)iei[8] = '00100000'B
. . . (Length)iel[1] = '10'O
. . . (BitStringType)aUTN[128] = '01010110010100010101000001010011010100100101110100000000000000000101010101010100010101110101011001010001010100000101001101010010'B
- Constraint:
ca_DataReq
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 00 05 12 00 55 55 55 55 55 55 55 55 55 55 55 55 55 55 55 55 20 10 56 51 50 53 52 5d 00 00 55 54 57 56 51 50 53 52

- No.: 904
- Timestamp: 10:52:14:057_0
- RFN: 1399
- Chip: 3584
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_MM_Authentication LINE 7
- Message Structure:
RRC_DataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain = 0
. (START_Value)start[0] = -
. AUTHENTICATIONRESPONSE
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)mMProtocolDiscriminator[4] = '0101'B
. . (MsgType)msgType[8] = '01010100'B
. . (AuthRsp)authRsp[32] = '01010101010101000101011101010110'B
. . AuthRspExt
- Constraint:
car_UplinkDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 00 05 54 55 54 57 56

- No.: 942
- Timestamp: 10:52:14:096_0
- RFN: 1403
- Chip: 768
- Event: Send
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_REQ
- Source: ts_SS_DownloadSecurityKey:lt_DownloadKeyCRLC LINE 1
- Message Structure:
CRLC_SecurityMode_Config_REQ
. (IntegerType)cellId = -1
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity = 0
. . (BitStringType)startValue[20] = "00000000000000000000"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = '01010111010101100101000101010000010100110101001001011101010111000101111101011110010110010101100001011011010110100101010101010100'B
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CRLC_SecurityModeCfgReq
- BinaryMessage:
30 21 02 01 ff 30 1c 0a 01 00 03 04 04 00 00 00 03 11 00 57 56 51 50 53 52 5d 5c 5f 5e 59 58 5b 5a 55 54

- No.: 943
- Timestamp: 10:52:14:098_0
- RFN: 1403
- Chip: 8192
- Event: Receive
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_CNF
- Source: ts_SS_DownloadSecurityKey:lt_DownloadKeyCRLC LINE 2
- Message Structure:
CRLC_SecurityMode_Config_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 950
- Timestamp: 10:52:14:105_0
- RFN: 1403
- Chip: 35840
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 1
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
. (IntegerType)count_I_LSB_UL = -
. (IntegerType)count_I_LSB_DL = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 00 02 01 00 02 01 00

- No.: 951
- Timestamp: 10:52:14:107_0
- RFN: 1404
- Chip: 5632
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 2
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 00 02 01 00

- No.: 952
- Timestamp: 10:52:14:109_0
- RFN: 1404
- Chip: 13056
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 3
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. (IntegerType)count_I_LSB_UL = -
. (IntegerType)count_I_LSB_DL = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 01 02 01 00

- No.: 953
- Timestamp: 10:52:14:111_0
- RFN: 1404
- Chip: 20224
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 4
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 954
- Timestamp: 10:52:14:113_0
- RFN: 1404
- Chip: 27904
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 5
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. (IntegerType)count_I_LSB_UL = -
. (IntegerType)count_I_LSB_DL = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 02 02 01 00

- No.: 955
- Timestamp: 10:52:14:115_0
- RFN: 1404
- Chip: 35328
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 6
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 956
- Timestamp: 10:52:14:117_0
- RFN: 1405
- Chip: 5120
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 7
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
. (IntegerType)count_I_LSB_UL = -
. (IntegerType)count_I_LSB_DL = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 03 02 01 00

- No.: 957
- Timestamp: 10:52:14:119_0
- RFN: 1405
- Chip: 12288
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 8
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 958
- Timestamp: 10:52:14:121_0
- RFN: 1405
- Chip: 19456
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 9
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
. (IntegerType)count_I_LSB_UL = -
. (IntegerType)count_I_LSB_DL = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 04 02 01 00

- No.: 959
- Timestamp: 10:52:14:123_0
- RFN: 1405
- Chip: 26624
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 10
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 963
- Timestamp: 10:52:14:154_0
- RFN: 1408
- Chip: 33024
- Event: Send
- PCO: CRLC
- Message: CRLC_Integrity_Activate_REQ
- Source: ts_CRLC_DL_Integrity LINE 1
- Message Structure:
CRLC_Integrity_Activate_REQ
. (IntegerType)cellId = -1
. (CN_DomainIdentity)cn_DomainIdentity = 0
. IntegrityActivationInfo
. . IntegrityProtectionModeInfo
. . . IntegrityProtectionModeCommand
. . . . startIntegrityProtection
. . . . . (BitStringType)integrityProtInitNumber[32] = "00000000000000000000000000000001"
. . . (IntegrityProtectionAlgorithm)integrityProtectionAlgorithm = 0
- Constraint:
ca_CRLC_DL_IntegrityActivateReq
- BinaryMessage:
30 15 02 01 ff 0a 01 00 30 0d 30 30 07 03 05 00 00 00 00 01 0a 01 00

- No.: 964
- Timestamp: 10:52:14:156_0
- RFN: 1409
- Chip: 1280
- Event: Receive
- PCO: CRLC
- Message: CRLC_Integrity_Activate_CNF
- Source: ts_CRLC_DL_Integrity LINE 2
- Message Structure:
CRLC_Integrity_Activate_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_IntegrityActivateCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 971
- Timestamp: 10:52:14:167_0
- RFN: 1410
- Chip: 3840
- Event: Send
- PCO: CRLC
- Message: CRLC_Integrity_Activate_REQ
- Source: ts_RB2_UL_IntegrityActivate LINE 1
- Message Structure:
CRLC_Integrity_Activate_REQ
. (IntegerType)cellId = -1
. (CN_DomainIdentity)cn_DomainIdentity = 0
. IntegrityActivationInfo
. . IntegrityProtActivationInfoList
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity = 2
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
- Constraint:
ca_CRLC_UL_IntegrityActivateReq
- BinaryMessage:
30 10 02 01 ff 0a 01 00 30 08 30 06 02 01 02 02 01 00

- No.: 972
- Timestamp: 10:52:14:169_0
- RFN: 1410
- Chip: 10496
- Event: Receive
- PCO: CRLC
- Message: CRLC_Integrity_Activate_CNF
- Source: ts_RB2_UL_IntegrityActivate LINE 2
- Message Structure:
CRLC_Integrity_Activate_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_IntegrityActivateCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 978
- Timestamp: 10:52:14:179_0
- RFN: 1411
- Chip: 12800
- Event: Send
- PCO: AM
- Message: RLC_AM_DATA_REQ
- Source: ts_RRC_Security:lt_SendSecurityModeCommand LINE 7
- Message Structure:
RLC_AM_DATA_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. AmConfirmationRequest
. aM_message
. . DL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00000000000000000000000000000000"
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . DL_DCCH_MessageType
. . . . SecurityModeCommand
. . . . . r3
. . . . . . SecurityModeCommand_r3_IEs
. . . . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . . . SecurityCapability
. . . . . . . . (BitStringType)cipheringAlgorithmCap[16] = '0000000000000011'B
. . . . . . . . (BitStringType)integrityProtectionAlgorithmCap[16] = '0000000000000010'B
. . . . . . . CipheringModeInfo
. . . . . . . IntegrityProtectionModeInfo
. . . . . . . . IntegrityProtectionModeCommand
. . . . . . . . . startIntegrityProtection
. . . . . . . . . . (BitStringType)integrityProtInitNumber[32] = "00000000000000000000000000000001"
. . . . . . . . (IntegrityProtectionAlgorithm)integrityProtectionAlgorithm = 0
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity = 0
. . . . . . . InterRAT_UE_SecurityCapList
. . . . . . laterNonCriticalExtensions
- Constraint:
cas_RRC_SecModeCmd
- BinaryMessage:
30 17 02 01 ff 02 01 02 05 00 80 00 00 00 04 04 00 01 80 01 40 00 00 00 20

- No.: 984
- Timestamp: 10:52:14:331_0
- RFN: 1426
- Chip: 18432
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_IND
- Source: ts_RRC_Security:lt_StartSecurity_UE LINE 8
- Message Structure:
RLC_AM_DATA_IND
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. IntegrityResult
. . (IntegrityStatus)integrityUsed = 0
. aM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "10000001100000001110110111011101"
. . . . (IntegerType)rrc_MessageSequenceNumber = 1
. . . UL_DCCH_MessageType
. . . . SecurityModeComplete
. . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . IntegrityProtActivationInfo
. . . . . . RRC_MessageSequenceNumberList
. . . . . . . (IntegerType)_elem = 0
. . . . . . . (IntegerType)_elem = 0
. . . . . . . (IntegerType)_elem = 0
. . . . . . . (IntegerType)_elem = 0
. . . . . . . (IntegerType)_elem = 0
. . . . . laterNonCriticalExtensions
. . . . . . (BitStringType)securityModeComplete_r3_add_ext = 0
. . . . . . nonCriticalExtensions
- Constraint:
car_RRC_SecModeCmpl
- BinaryMessage:
30 12 02 01 ff 02 01 02 0a 01 00 c0 c0 76 ee 8d 21 00 00 00

- No.: 985
- Timestamp: 10:52:14:332_0
- RFN: 1426
- Chip: 22784
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_Security:lt_StartSecurity_UE LINE 8
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 987
- Timestamp: 10:52:14:336_0
- RFN: 1427
- Chip: 768
- Event: Send
- PCO: CRLC
- Message: CRLC_Integrity_Activate_REQ
- Source: ts_CRLC_UL_Integrity LINE 1
- Message Structure:
CRLC_Integrity_Activate_REQ
. (IntegerType)cellId = -1
. (CN_DomainIdentity)cn_DomainIdentity = 0
. IntegrityActivationInfo
. . IntegrityProtActivationInfoList
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity = 0
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity = 1
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity = 3
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity = 4
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
- Constraint:
ca_CRLC_UL_IntegrityActivateReq
- BinaryMessage:
30 28 02 01 ff 0a 01 00 30 20 30 06 02 01 00 02 01 00 30 06 02 01 01 02 01 00 30 06 02 01 03 02 01 00 30 06 02 01 04 02 01 00

- No.: 988
- Timestamp: 10:52:14:338_0
- RFN: 1427
- Chip: 8448
- Event: Receive
- PCO: CRLC
- Message: CRLC_Integrity_Activate_CNF
- Source: ts_CRLC_UL_Integrity LINE 2
- Message Structure:
CRLC_Integrity_Activate_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_IntegrityActivateCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 995
- Timestamp: 10:52:14:358_0
- RFN: 1429
- Chip: 7424
- Event: Send
- PCO: Dc
- Message: RRC_DataReq
- Source: ts_GMM_IdleUpdated:lt_LocUpdAcc LINE 2
- Message Structure:
RRC_DataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[-1] = -
. (SapId)sapId[1] = -
. (SS_CN_DomainIdentity)cN_Domain = 0
. LOCATIONUPDATINGACCEPT
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)mMProtocolDiscriminator[4] = '0101'B
. . (MsgType)msgType[8] = '00000010'B
. . LocAreaId_v
. . . (OctetStringType)plmn[3] = '00F110'O
. . . (OctetStringType)lac[2] = '0001'O
. . MM_MS_Identity
. . . (IEI8)iei[8] = '00010111'B
. . . (Length)iel[1] = '05'O
. . . (B4)iDigit1[4] = '1111'B
. . . (B1)oddEvenInd[1] = '0'B
. . . (B3)typeOfId[3] = '100'B
. . . (OctetStringType)otherDigits[-1] = '12345678'O
. . (FollowOnProceed)followOnProceed[8] = '10100001'B
. . (CTSPerm)cTSPerm[8] = '10100010'B
. . PLMN_List
- Constraint:
ca_DataReq
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 00 05 02 00 f1 10 00 01 17 05 f4 12 34 56 78 a1 a2

- No.: 999
- Timestamp: 10:52:14:507_0
- RFN: 1444
- Chip: 5632
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_GMM_IdleUpdated:lt_LocUpdAcc LINE 3
- Message Structure:
RRC_DataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain = 0
. (START_Value)start[0] = -
. TMSIREALLOCATIONCOMPLETE
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)mMProtocolDiscriminator[4] = '0101'B
. . (MsgType)msgType[8] = '10011011'B
- Constraint:
car_UplinkDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 00 05 9b

- No.: 1013
- Timestamp: 10:52:14:518_1
- RFN: 1445
- Chip: 9216
- Event: Start Timer
- Source: ts_RRC_Delay LINE 1
- Message Structure:
no details available
- Constraint:
t_Dly (1000 Ms)
- BinaryMessage:

- No.: 1017
- Timestamp: 10:52:15:510_0
- RFN: 1544
- Chip: 17664
- Event: Timeout
- Source: ts_RRC_Delay LINE 2
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 1022
- Timestamp: 10:52:15:516_0
- RFN: 1545
- Chip: 2304
- Event: Send
- PCO: UM
- Message: RLC_UM_DATA_REQ
- Source: ts_RRC_ConnRel:lt_Send_RRC_ConnectionRelease LINE 3
- Message Structure:
RLC_UM_DATA_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. uM_message
. . DL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00000000000000000000000000000000"
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . DL_DCCH_MessageType
. . . . RRCConnectionRelease
. . . . . r3
. . . . . . RRCConnectionRelease_r3_IEs
. . . . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . . . (IntegerType)n_308 = 1
. . . . . . . (ReleaseCause)releaseCause = 0
. . . . . . . Rplmn_Information
. . . . . . laterNonCriticalExtensions
. (BooleanType)specialLI = FALSE
- Constraint:
cas_RRC_ConnRelDCCH
- BinaryMessage:
30 10 02 01 ff 02 01 01 80 00 00 00 03 c8 00 01 01 00

- No.: 1026
- Timestamp: 10:52:15:649_0
- RFN: 1558
- Chip: 9728
- Event: Receive
- PCO: UM
- Message: RLC_UM_DATA_IND
- Source: ts_RRC_ConnRel:lt_Send_RRC_ConnectionRelease LINE 4
- Message Structure:
RLC_UM_DATA_IND
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. IntegrityResult
. uM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "10101101101011101001000000111001"
. . . . (IntegerType)rrc_MessageSequenceNumber = 1
. . . UL_DCCH_MessageType
. . . . RRCConnectionReleaseComplete
. . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . FailureCauseWithProtErr
. . . . . laterNonCriticalExtensions
. . . . . . (BitStringType)rrcConnectionReleaseComplete_r3_add_ext = 0
. . . . . . nonCriticalExtensions
- Constraint:
car_RRC_ConnRelCmplUM
- BinaryMessage:
30 0c 02 01 ff 02 01 01 d6 d7 48 1c 8c 40

- No.: 1027
- Timestamp: 10:52:15:650_0
- RFN: 1558
- Chip: 13312
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ConnRel:lt_Send_RRC_ConnectionRelease LINE 4
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1030
- Timestamp: 10:52:15:651_0
- RFN: 1558
- Chip: 18176
- Event: Start Timer
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 1
- Message Structure:
no details available
- Constraint:
t_Dly (5000 Ms)
- BinaryMessage:

- No.: 1034
- Timestamp: 10:52:15:797_0
- RFN: 1573
- Chip: 7168
- Event: Receive
- PCO: UM
- Message: RLC_UM_DATA_IND
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 4
- Message Structure:
RLC_UM_DATA_IND
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. IntegrityResult
. uM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00011100010101000111110101101001"
. . . . (IntegerType)rrc_MessageSequenceNumber = 2
. . . UL_DCCH_MessageType
. . . . RRCConnectionReleaseComplete
. . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . FailureCauseWithProtErr
. . . . . laterNonCriticalExtensions
. . . . . . (BitStringType)rrcConnectionReleaseComplete_r3_add_ext = 0
. . . . . . nonCriticalExtensions
- Constraint:
car_RRC_ConnRelCmplUM
- BinaryMessage:
30 0c 02 01 ff 02 01 01 8e 2a 3e b4 94 40

- No.: 1035
- Timestamp: 10:52:15:798_0
- RFN: 1573
- Chip: 11264
- Event: Cancel Timer
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 4
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 1036
- Timestamp: 10:52:15:799_0
- RFN: 1573
- Chip: 12288
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 4
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1042
- Timestamp: 10:52:15:803_0
- RFN: 1573
- Chip: 27648
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 01 0a 01 00 05 00

- No.: 1046
- Timestamp: 10:52:15:809_0
- RFN: 1574
- Chip: 13568
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 1049
- Timestamp: 10:52:15:812_0
- RFN: 1574
- Chip: 25344
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 02 0a 01 00 05 00

- No.: 1053
- Timestamp: 10:52:15:819_0
- RFN: 1575
- Chip: 14336
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 1056
- Timestamp: 10:52:15:822_0
- RFN: 1575
- Chip: 26112
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 03 0a 01 00 05 00

- No.: 1060
- Timestamp: 10:52:15:834_0
- RFN: 1576
- Chip: 32512
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 1063
- Timestamp: 10:52:15:837_0
- RFN: 1577
- Chip: 5120
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 04 0a 01 00 05 00

- No.: 1067
- Timestamp: 10:52:15:846_0
- RFN: 1578
- Chip: 3328
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 1070
- Timestamp: 10:52:15:854_0
- RFN: 1578
- Chip: 32256
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 136
. . . . . UL_RLC_Mode
. . . . . . UL_UM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (NoExplicitDiscard)timerBasedNoExplicit = 9
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = 1
. . . . (IntegerType)dLlogicalChannelIdentity = 1
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_UM_Info
- BinaryMessage:
30 22 02 01 ff 02 01 01 0a 01 00 30 17 30 0d 05 00 30 09 02 02 00 88 30 03 0a 01 09 30 06 02 01 01 02 01 01

- No.: 1074
- Timestamp: 10:52:15:864_0
- RFN: 1579
- Chip: 33024
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 1075
- Timestamp: 10:52:15:872_0
- RFN: 1580
- Chip: 26112
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 3
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . (TimerEPC)timerEPC = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . (TimerRST)timerRST = 9
. . . . . . . (MaxRST)max_RST = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = 2
. . . . (IntegerType)dLlogicalChannelIdentity = 2
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 02 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 27 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 02 02 01 02

- No.: 1079
- Timestamp: 10:52:15:894_0
- RFN: 1582
- Chip: 28928
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 4
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 1080
- Timestamp: 10:52:15:903_0
- RFN: 1583
- Chip: 24320
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 5
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . (TimerEPC)timerEPC = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . (TimerRST)timerRST = 9
. . . . . . . (MaxRST)max_RST = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = 3
. . . . (IntegerType)dLlogicalChannelIdentity = 3
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 03 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 27 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 03 02 01 03

- No.: 1084
- Timestamp: 10:52:15:916_0
- RFN: 1585
- Chip: 768
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 6
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 1085
- Timestamp: 10:52:15:926_0
- RFN: 1585
- Chip: 36352
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 7
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . (TimerEPC)timerEPC = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . (TimerRST)timerRST = 9
. . . . . . . (MaxRST)max_RST = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = 4
. . . . (IntegerType)dLlogicalChannelIdentity = 4
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 04 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 27 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 04 02 01 04

- No.: 1089
- Timestamp: 10:52:15:945_0
- RFN: 1587
- Chip: 33792
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 8
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 1112
- Timestamp: 10:52:15:954_1
- RFN: 1588
- Chip: 30464
- Event: Start Timer
- Source: ts_GMM_IdleUpdated:lt_HandleAttachRequest LINE 5
- Message Structure:
no details available
- Constraint:
t_WaitS (1 Sec)
- BinaryMessage:

- No.: 1116
- Timestamp: 10:52:16:955_0
- RFN: 1688
- Chip: 35328
- Event: Timeout
- Source: ts_GMM_IdleUpdated:lt_HandleAttachRequest LINE 6
- Message Structure:
no details available
- Constraint:
t_WaitS
- BinaryMessage:

- No.: 1118
- Timestamp: 10:52:16:956_1
- RFN: 1689
- Chip: 256
- Event: Start Timer
- Source: ts_GMM_IdleUpdated:lt_HandleAttachRequest LINE 7
- Message Structure:
no details available
- Constraint:
t_WaitS (60 Sec)
- BinaryMessage:

- No.: 1120
- Timestamp: 10:52:16:958_0
- RFN: 1689
- Chip: 8448
- Event: Send
- PCO: Ut
- Message: AT_CmdReq
- Source: ts_AT_TriggerGMM_Attach LINE 1
- Message Structure:
AT_CmdReq
. (IA5StringType)cmd[-1] = "AT+CGATT=1"
. (HexStringType)sMS_BlockMode[-1] = -
- Constraint:
ca_AT_CmdReq
- BinaryMessage:
41 54 2b 43 47 41 54 54 3d 31 3c 43 52 3e

- No.: 1124
- Timestamp: 10:52:18:095_0
- RFN: 1802
- Chip: 33536
- Event: Receive
- PCO: Ut
- Message: AT_CmdCnf
- Source: ts_AT_TriggerGMM_Attach LINE 2
- Message Structure:
AT_CmdCnf
. (BooleanType)result = TRUE
. (IA5StringType)resultString[18] = "OK"
. (HexStringType)sMS_BlockMode[0] = -
- Constraint:
ca_AT_CmdCnf
- BinaryMessage:
80 3c 43 52 3e 3c 4c 46 3e 4f 4b 3c 43 52 3e 3c 4c 46 3e

- No.: 1141
- Timestamp: 10:52:18:102_0
- RFN: 1803
- Chip: 22016
- Event: Receive
- PCO: CPHY
- Message: CPHY_Out_of_Sync_IND
- Source: RRC_DefConnEst LINE 7
- Message Structure:
CPHY_Out_of_Sync_IND
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_OutOfSyncInd
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 1142
- Timestamp: 10:52:18:103_0
- RFN: 1803
- Chip: 24064
- Event: Cancel Timer
- Source: RRC_DefConnEst LINE 7
- Message Structure:
no details available
- Constraint:
t_T312
- BinaryMessage:

- No.: 1143
- Timestamp: 10:52:18:103_1
- RFN: 1803
- Chip: 26112
- Event: Default
- Source: RRC_DefConnEst LINE 0
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1144
- Timestamp: 10:52:18:103_2
- RFN: 1803
- Chip: 27136
- Event: Default
- Source: ts_RRC_ConnEst:lt_RcvConnReq LINE 2
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1149
- Timestamp: 10:52:19:672_0
- RFN: 1960
- Chip: 20480
- Event: Receive
- PCO: TM
- Message: RLC_TR_DATA_IND
- Source: ts_RRC_ConnEst:lt_RcvConnReq LINE 2
- Message Structure:
RLC_TR_DATA_IND
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
. tM_message
. . UL_CCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode = 0
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . UL_CCCH_MessageType
. . . . RRCConnectionRequest
. . . . . InitialUE_Identity
. . . . . . TMSI_and_LAI_GSM_MAP
. . . . . . . (BitStringType)tmsi[32] = "00010010001101000101011001111000"
. . . . . . . LAI
. . . . . . . . PLMN_Identity
. . . . . . . . . MCC
. . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . (IntegerType)_elem = 1
. . . . . . . . . MNC
. . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . (IntegerType)_elem = 1
. . . . . . . . (BitStringType)lac[16] = '0000000000000001'B
. . . . . (EstablishmentCause)establishmentCause = 12
. . . . . (ProtocolErrorIndicator)protocolErrorIndicator = 0
. . . . . MeasuredResultsOnRACH
. . . . . . currentCell
. . . . . . . modeSpecificInfo
. . . . . . . . fdd
. . . . . . . . . measurementQuantity
. . . . . . . . . . (IntegerType)cpich_Ec_N0 = 0
. . . . . v3d0NonCriticalExtensions
. . . . . . RRCConnectionRequest_v3d0ext_IEs
. . . . . . . (BitStringType)uESpecificBehaviourInformation1idle = 0
. . . . . . nonCriticalExtensions
- Constraint:
car_RRC_ConnReq
- BinaryMessage:
30 11 02 01 00 02 01 00 21 12 34 56 78 00 10 08 00 0b 00

- No.: 1153
- Timestamp: 10:52:19:733_0
- RFN: 1966
- Chip: 26368
- Event: Send
- PCO: UM
- Message: RLC_UM_DATA_REQ
- Source: ts_RRC_ConnEst:lt_Send_ConnSetUp LINE 22
- Message Structure:
RLC_UM_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
. uM_message
. . DL_CCCH_Message
. . . IntegrityCheckInfo
. . . DL_CCCH_MessageType
. . . . RRCConnectionSetup
. . . . . r3
. . . . . . RRCConnectionSetup_r3_IEs
. . . . . . . InitialUE_Identity
. . . . . . . . TMSI_and_LAI_GSM_MAP
. . . . . . . . . (BitStringType)tmsi[32] = "00010010001101000101011001111000"
. . . . . . . . . LAI
. . . . . . . . . . PLMN_Identity
. . . . . . . . . . . MCC
. . . . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . . . (IntegerType)_elem = 1
. . . . . . . . . . . MNC
. . . . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . . . (IntegerType)_elem = 1
. . . . . . . . . . (BitStringType)lac[16] = '0000000000000001'B
. . . . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . . . (IntegerType)activationTime = -
. . . . . . . U_RNTI
. . . . . . . . (BitStringType)srnc_Identity[12] = "000000000001"
. . . . . . . . (BitStringType)s_RNTI[20] = "00000000000000000001"
. . . . . . . (BitStringType)new_c_RNTI[16] = -
. . . . . . . (RRC_StateIndicator)rrc_StateIndicator = 0
. . . . . . . (IntegerType)utran_DRX_CycleLengthCoeff = 9
. . . . . . . CapabilityUpdateRequirement
. . . . . . . . (BooleanType)ue_RadioCapabilityFDDUpdateRequirement = TRUE
. . . . . . . . (BooleanType)ue_RadioCapabilityTDDUpdateRequirement = FALSE
. . . . . . . . SystemSpecificCapUpdateReqList
. . . . . . . . . (SystemSpecificCapUpdateReq)_elem = 0
. . . . . . . SRB_InformationSetupList2
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_UM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 1
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 1
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . . . . . . . (TimerRST)timerRST = 9
. . . . . . . . . . . . . (MaxRST)max_RST = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 2
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 2
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . . . . . . . (TimerRST)timerRST = 9
. . . . . . . . . . . . . (MaxRST)max_RST = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 3
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 3
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . . . . . . . (TimerRST)timerRST = 9
. . . . . . . . . . . . . (MaxRST)max_RST = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 4
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 4
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . UL_CommonTransChInfo
. . . . . . . . TFC_Subset
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . TFCS
. . . . . . . . . . . ExplicitTFCS_Configuration
. . . . . . . . . . . . TFCS_ReconfAdd
. . . . . . . . . . . . . ctfcSize
. . . . . . . . . . . . . . ctfc2Bit
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . . . . . . . (IntegerType)ctfc2 = 0
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . . . . . . . (IntegerType)ctfc2 = 1
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 11
. . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . UL_AddReconfTransChInfoList
. . . . . . . . UL_AddReconfTransChInformation
. . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType = 0
. . . . . . . . . (IntegerType)transportChannelIdentity = 5
. . . . . . . . . TransportFormatSet
. . . . . . . . . . DedicatedTransChTFS
. . . . . . . . . . . tti
. . . . . . . . . . . . DedicatedDynamicTF_InfoList
. . . . . . . . . . . . . DedicatedDynamicTF_Info
. . . . . . . . . . . . . . rlc_Size
. . . . . . . . . . . . . . . BitModeRLC_SizeInfo
. . . . . . . . . . . . . . . . sizeType2
. . . . . . . . . . . . . . . . . (IntegerType)part1 = 2
. . . . . . . . . . . . . . . . . (IntegerType)part2 = -
. . . . . . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . LogicalChannelList
. . . . . . . . . . . SemistaticTF_Information
. . . . . . . . . . . . ChannelCodingType
. . . . . . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . . . . . (IntegerType)rateMatchingAttribute = 192
. . . . . . . . . . . . (CRC_Size)crc_Size = 3
. . . . . . . DL_CommonTransChInfo
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . dl_Parameters
. . . . . . . DL_AddReconfTransChInfoList
. . . . . . . . DL_AddReconfTransChInformation
. . . . . . . . . (DL_TrCH_Type)dl_TransportChannelType = 0
. . . . . . . . . (IntegerType)dl_transportChannelIdentity = 10
. . . . . . . . . tfs_SignallingMode
. . . . . . . . . . UL_TransportChannelIdentity
. . . . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType = 0
. . . . . . . . . . . (IntegerType)ul_TransportChannelIdentity = 5
. . . . . . . . . QualityTarget
. . . . . . . . . . (IntegerType)bler_QualityValue = -20
. . . . . . . . . TM_SignallingInfo
. . . . . . . FrequencyInfo
. . . . . . . (IntegerType)maxAllowedUL_TX_Power = -
. . . . . . . UL_ChannelRequirement
. . . . . . . . UL_DPCH_Info
. . . . . . . . . UL_DPCH_PowerControlInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (IntegerType)dpcch_PowerOffset = -40
. . . . . . . . . . . (IntegerType)pc_Preamble = 1
. . . . . . . . . . . (IntegerType)sRB_delay = 7
. . . . . . . . . . . PowerControlAlgorithm
. . . . . . . . . . . . (IntegerType)algorithm1 = 1
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (ScramblingCodeType)scramblingCodeType = 1
. . . . . . . . . . . (IntegerType)scramblingCode = 0
. . . . . . . . . . . (IntegerType)numberOfDPDCH = -
. . . . . . . . . . . (SpreadingFactor)spreadingFactor = 4
. . . . . . . . . . . (BooleanType)tfci_Existence = TRUE
. . . . . . . . . . . (IntegerType)numberOfFBI_Bits = -
. . . . . . . . . . . (PuncturingLimit)puncturingLimit = 15
. . . . . . . DL_CommonInformation
. . . . . . . . DL_DPCH_InfoCommon
. . . . . . . . . cfnHandling
. . . . . . . . . . initialise
. . . . . . . . . . . (IntegerType)cfntargetsfnframeoffset = -
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . DL_DPCH_PowerControlInfo
. . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . (DPC_Mode)dpc_Mode = 0
. . . . . . . . . . . (IntegerType)powerOffsetPilot_pdpdch = 0
. . . . . . . . . . . Dl_rate_matching_restriction
. . . . . . . . . . . SF512_AndPilot
. . . . . . . . . . . . (PilotBits128)sfd128 = 0
. . . . . . . . . . . (PositionFixedOrFlexible)positionFixedOrFlexible = 0
. . . . . . . . . . . (BooleanType)tfci_Existence = FALSE
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . (IntegerType)defaultDPCH_OffsetValue = 0
. . . . . . . . . . DPCH_CompressedModeInfo
. . . . . . . . . . (TX_DiversityMode)tx_DiversityMode = 0
. . . . . . . . . . SSDT_Information
. . . . . . . DL_InformationPerRL_List
. . . . . . . . DL_InformationPerRL
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . PrimaryCPICH_Info
. . . . . . . . . . . . (IntegerType)primaryScramblingCode = 100
. . . . . . . . . . . PDSCH_SHO_DCH_Info
. . . . . . . . . . . PDSCH_CodeMapping
. . . . . . . . . DL_DPCH_InfoPerRL
. . . . . . . . . . fdd
. . . . . . . . . . . (PCPICH_UsageForChannelEst)pCPICH_UsageForChannelEst = 0
. . . . . . . . . . . (IntegerType)dpch_FrameOffset = 0
. . . . . . . . . . . SecondaryCPICH_Info
. . . . . . . . . . . DL_ChannelisationCodeList
. . . . . . . . . . . . DL_ChannelisationCode
. . . . . . . . . . . . . (IntegerType)secondaryScramblingCode = 1
. . . . . . . . . . . . . SF512_AndCodeNumber
. . . . . . . . . . . . . . (IntegerType)sf128 = 0
. . . . . . . . . . . . . (ScramblingCodeChange)scramblingCodeChange = 1
. . . . . . . . . . . (IntegerType)tpc_CombinationIndex = 0
. . . . . . . . . . . (SSDT_CellIdentity)ssdt_CellIdentity = -
. . . . . . . . . . . (ClosedLoopTimingAdjMode)closedLoopTimingAdjMode = -
. . . . . . . . . SCCPCH_InfoForFACH
. . . . . . laterNonCriticalExtensions
. (BooleanType)specialLI = TRUE
- Constraint:
cas_RRC_ConnSetup
- BinaryMessage:
30 78 02 01 00 02 01 00 30 e7 22 46 8a cf 00 02 01 00 01 00 04 00 00 4d 82 69 3a 10 10 89 0d 42 00 02 81 9e 8e 46 c9 ce 7c 9c 4e 74 20 a5 12 3a 8c 00 15 13 3d 1c 8d 93 9c f9 38 9c e8 42 52 24 b5 28 00 4a 46 7a 39 1b 27 39 f2 71 39 d0 86 b4 49 ea 70 00 d4 c8 00 06 25 2b f0 02 00 08 82 23 bf 66 08 98 95 a5 47 a2 00 00 01 3f 90 0a 14 00 02 06 40 00 0c 28 08 01 01 ff

- No.: 1174
- Timestamp: 10:52:19:776_1
- RFN: 1971
- Chip: 256
- Event: Start Timer
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 3
- Message Structure:
no details available
- Constraint:
t_WaitMS (13500 Ms)
- BinaryMessage:

- No.: 1179
- Timestamp: 10:52:19:994_0
- RFN: 1992
- Chip: 29696
- Event: Receive
- PCO: CPHY
- Message: CPHY_Sync_IND
- Source: RRC_Def1 LINE 13
- Message Structure:
CPHY_Sync_IND
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_SyncInd
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 1180
- Timestamp: 10:52:19:994_1
- RFN: 1992
- Chip: 31488
- Event: Cancel Timer
- Source: RRC_Def1 LINE 13
- Message Structure:
no details available
- Constraint:
t_T312
- BinaryMessage:

- No.: 1181
- Timestamp: 10:52:19:995_0
- RFN: 1992
- Chip: 33280
- Event: Default
- Source: RRC_Def1 LINE 0
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1182
- Timestamp: 10:52:19:995_1
- RFN: 1992
- Chip: 34048
- Event: Default
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1187
- Timestamp: 10:52:20:109_0
- RFN: 2004
- Chip: 14080
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_IND
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
RLC_AM_DATA_IND
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. IntegrityResult
. . (IntegrityStatus)integrityUsed = 0
. aM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode = 0
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . UL_DCCH_MessageType
. . . . RRCConnectionSetupComplete
. . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . STARTList
. . . . . . STARTSingle
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity = 1
. . . . . . . (BitStringType)start_Value[20] = "00000000000000000100"
. . . . . . STARTSingle
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity = 0
. . . . . . . (BitStringType)start_Value[20] = "00000000000000000010"
. . . . . UE_RadioAccessCapability
. . . . . . (AccessStratumReleaseIndicator)accessStratumReleaseIndicator = 0
. . . . . . PDCP_Capability
. . . . . . . (BooleanType)losslessSRNS_RelocationSupport = FALSE
. . . . . . . supportForRfc2507
. . . . . . RLC_Capability
. . . . . . . (TotalRLC_AM_BufferSize)totalRLC_AM_BufferSize = 2
. . . . . . . (MaximumRLC_WindowSize)maximumRLC_WindowSize = 0
. . . . . . . (MaximumAM_EntityNumberRLC_Cap)maximumAM_EntityNumber = 3
. . . . . . TransportChannelCapability
. . . . . . . DL_TransChCapability
. . . . . . . . (MaxNoBits)maxNoBitsReceived = 4
. . . . . . . . (MaxNoBits)maxConvCodeBitsReceived = 1
. . . . . . . . TurboSupport
. . . . . . . . . (MaxNoBits)supported = 4
. . . . . . . . (MaxSimultaneousTransChsDL)maxSimultaneousTransChs = 1
. . . . . . . . (IntegerType)maxSimultaneousCCTrCH_Count = 1
. . . . . . . . (MaxTransportBlocksDL)maxReceivedTransportBlocks = 2
. . . . . . . . (MaxNumberOfTFC_DL)maxNumberOfTFC = 4
. . . . . . . . (MaxNumberOfTF)maxNumberOfTF = 1
. . . . . . . UL_TransChCapability
. . . . . . . . (MaxNoBits)maxNoBitsTransmitted = 3
. . . . . . . . (MaxNoBits)maxConvCodeBitsTransmitted = 1
. . . . . . . . TurboSupport
. . . . . . . . . (MaxNoBits)supported = 3
. . . . . . . . (MaxSimultaneousTransChsUL)maxSimultaneousTransChs = 2
. . . . . . . . modeSpecificInfo
. . . . . . . . (MaxTransportBlocksUL)maxTransmittedBlocks = 2
. . . . . . . . (MaxNumberOfTFC_UL)maxNumberOfTFC = 3
. . . . . . . . (MaxNumberOfTF)maxNumberOfTF = 0
. . . . . . RF_Capability
. . . . . . . fddRF_Capability
. . . . . . . . (IntegerType)ue_PowerClass = 4
. . . . . . . . (TxRxFrequencySeparation)txRxFrequencySeparation = 0
. . . . . . . tddRF_Capability
. . . . . . . . (IntegerType)ue_PowerClass = 0
. . . . . . . . (RadioFrequencyBandTDDList)radioFrequencyTDDBandList = 0
. . . . . . . . (ChipRateCapability)chipRateCapability = 0
. . . . . . PhysicalChannelCapability
. . . . . . . fddPhysChCapability
. . . . . . . . DL_PhysChCapabilityFDD
. . . . . . . . . (IntegerType)maxNoDPCH_PDSCH_Codes = 3
. . . . . . . . . (MaxNoPhysChBitsReceived)maxNoPhysChBitsReceived = 6
. . . . . . . . . (BooleanType)supportForSF_512 = FALSE
. . . . . . . . . (BooleanType)supportOfPDSCH = FALSE
. . . . . . . . . SimultaneousSCCPCH_DPCH_Reception
. . . . . . . . UL_PhysChCapabilityFDD
. . . . . . . . . (MaxNoDPDCH_BitsTransmitted)maxNoDPDCH_BitsTransmitted = 2
. . . . . . . . . (BooleanType)supportOfPCPCH = FALSE
. . . . . . . tddPhysChCapability
. . . . . . . . DL_PhysChCapabilityTDD
. . . . . . . . . (IntegerType)maxTS_PerFrame = 0
. . . . . . . . . (IntegerType)maxPhysChPerFrame = 0
. . . . . . . . . (MinimumSF_DL)minimumSF = 0
. . . . . . . . . (BooleanType)supportOfPDSCH = FALSE
. . . . . . . . . (IntegerType)maxPhysChPerTS = 0
. . . . . . . . UL_PhysChCapabilityTDD
. . . . . . . . . (IntegerType)maxTS_PerFrame = 0
. . . . . . . . . (MaxPhysChPerTimeslot)maxPhysChPerTimeslot = 0
. . . . . . . . . (MinimumSF_UL)minimumSF = 0
. . . . . . . . . (BooleanType)supportOfPUSCH = FALSE
. . . . . . UE_MultiModeRAT_Capability
. . . . . . . MultiRAT_Capability
. . . . . . . . (BooleanType)supportOfGSM = TRUE
. . . . . . . . (BooleanType)supportOfMulticarrier = FALSE
. . . . . . . (MultiModeCapability)multiModeCapability = 1
. . . . . . SecurityCapability
. . . . . . . (BitStringType)cipheringAlgorithmCap[16] = '0000000000000011'B
. . . . . . . (BitStringType)integrityProtectionAlgorithmCap[16] = '0000000000000010'B
. . . . . . UE_Positioning_Capability
. . . . . . . (BooleanType)standaloneLocMethodsSupported = FALSE
. . . . . . . (BooleanType)ue_BasedOTDOA_Supported = FALSE
. . . . . . . (NetworkAssistedGPS_Supported)networkAssistedGPS_Supported = 3
. . . . . . . (BooleanType)supportForUE_GPS_TimingOfCellFrames = FALSE
. . . . . . . (BooleanType)supportForIPDL = FALSE
. . . . . . MeasurementCapability
. . . . . . . CompressedModeMeasCapability
. . . . . . . . (BooleanType)fdd_Measurements = TRUE
. . . . . . . . (BooleanType)tdd_Measurements = FALSE
. . . . . . . . GSM_Measurements
. . . . . . . . . (BooleanType)gsm900 = TRUE
. . . . . . . . . (BooleanType)dcs1800 = TRUE
. . . . . . . . . (BooleanType)gsm1900 = FALSE
. . . . . . . . (BooleanType)multiCarrierMeasurements = FALSE
. . . . . . . CompressedModeMeasCapability
. . . . . . . . (BooleanType)fdd_Measurements = TRUE
. . . . . . . . (BooleanType)tdd_Measurements = FALSE
. . . . . . . . GSM_Measurements
. . . . . . . . . (BooleanType)gsm900 = TRUE
. . . . . . . . . (BooleanType)dcs1800 = TRUE
. . . . . . . . . (BooleanType)gsm1900 = FALSE
. . . . . . . . (BooleanType)multiCarrierMeasurements = FALSE
. . . . . v370NonCriticalExtensions
. . . . . . RRCConnectionSetupComplete_v370ext
. . . . . . . UE_RadioAccessCapability_v370ext
. . . . . . v380NonCriticalExtensions
. . . . . . . RRCConnectionSetupComplete_v380ext_IEs
. . . . . . . . UE_RadioAccessCapability_v380ext
. . . . . . . . . UE_PositioningCapabilityExt_v380
. . . . . . . . . . (BooleanType)rx_tx_TimeDifferenceType2Capable = FALSE
. . . . . . . . DL_PhysChCapabilityFDD_v380ext
. . . . . . . . . (SupportOfDedicatedPilotsForChEstimation)supportOfDedicatedPilotsForChEstimation = 0
. . . . . . . v3a0NonCriticalExtensions
. . . . . . . . RRCConnectionSetupComplete_v3a0ext_IEs
. . . . . . . . . UE_RadioAccessCapability_v3a0ext
. . . . . . . . . . UE_PositioningCapabilityExt_v3a0
. . . . . . . . . . . (UE_PositioningCapabilityExt_v3a0_list_0)validity_CellPCH_UraPCH = 0
. . . . . . . . laterNonCriticalExtensions
. . . . . . . . . (BitStringType)rrcConnectionSetupComplete_r3_add_ext = 0
. . . . . . . . . nonCriticalExtensions
- Constraint:
car_RRC_ConnSetupCmpl
- BinaryMessage:
30 27 02 01 ff 02 01 02 0a 05 01 00 00 00 00 4a 0c 00 01 00 00 05 11 a0 d1 04 84 c6 68 46 2c 93 02 48 00 18 00 11 8f 8f 80

- No.: 1188
- Timestamp: 10:52:20:117_0
- RFN: 2005
- Chip: 5120
- Event: Cancel Timer
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
t_WaitMS
- BinaryMessage:

- No.: 1189
- Timestamp: 10:52:20:117_1
- RFN: 2005
- Chip: 6144
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1203
- Timestamp: 10:52:20:126_0
- RFN: 2006
- Chip: 1536
- Event: Send
- PCO: CMAC
- Message: CMAC_SecurityMode_Config_REQ
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 1
- Message Structure:
CMAC_SecurityMode_Config_REQ
. (IntegerType)cellId = 0
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity = 1
. . (BitStringType)startValue[20] = "00000000000000000100"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = -
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CMAC_SecurityModeCfgReq
- BinaryMessage:
30 0e 02 01 00 30 09 0a 01 01 03 04 04 00 00 40

- No.: 1204
- Timestamp: 10:52:20:128_0
- RFN: 2006
- Chip: 10240
- Event: Receive
- PCO: CMAC
- Message: CMAC_SecurityMode_Config_CNF
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 2
- Message Structure:
CMAC_SecurityMode_Config_CNF
. (IntegerType)cellId = 0
- Constraint:
ca_CMAC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 00

- No.: 1205
- Timestamp: 10:52:20:130_0
- RFN: 2006
- Chip: 17152
- Event: Send
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_REQ
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 3
- Message Structure:
CRLC_SecurityMode_Config_REQ
. (IntegerType)cellId = -1
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity = 1
. . (BitStringType)startValue[20] = "00000000000000000100"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = -
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CRLC_SecurityModeCfgReq
- BinaryMessage:
30 0e 02 01 ff 30 09 0a 01 01 03 04 04 00 00 40

- No.: 1206
- Timestamp: 10:52:20:132_0
- RFN: 2006
- Chip: 23296
- Event: Receive
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_CNF
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 4
- Message Structure:
CRLC_SecurityMode_Config_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1220
- Timestamp: 10:52:20:137_0
- RFN: 2007
- Chip: 4864
- Event: Send
- PCO: CMAC
- Message: CMAC_SecurityMode_Config_REQ
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 1
- Message Structure:
CMAC_SecurityMode_Config_REQ
. (IntegerType)cellId = 0
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity = 0
. . (BitStringType)startValue[20] = "00000000000000000010"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = -
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CMAC_SecurityModeCfgReq
- BinaryMessage:
30 0e 02 01 00 30 09 0a 01 00 03 04 04 00 00 20

- No.: 1221
- Timestamp: 10:52:20:139_0
- RFN: 2007
- Chip: 11008
- Event: Receive
- PCO: CMAC
- Message: CMAC_SecurityMode_Config_CNF
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 2
- Message Structure:
CMAC_SecurityMode_Config_CNF
. (IntegerType)cellId = 0
- Constraint:
ca_CMAC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 00

- No.: 1222
- Timestamp: 10:52:20:140_0
- RFN: 2007
- Chip: 18432
- Event: Send
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_REQ
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 3
- Message Structure:
CRLC_SecurityMode_Config_REQ
. (IntegerType)cellId = -1
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity = 0
. . (BitStringType)startValue[20] = "00000000000000000010"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = -
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CRLC_SecurityModeCfgReq
- BinaryMessage:
30 0e 02 01 ff 30 09 0a 01 00 03 04 04 00 00 20

- No.: 1223
- Timestamp: 10:52:20:142_0
- RFN: 2007
- Chip: 24576
- Event: Receive
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_CNF
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 4
- Message Structure:
CRLC_SecurityMode_Config_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1230
- Timestamp: 10:52:20:168_0
- RFN: 2010
- Chip: 7936
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_GMM_IdleUpdated:lt_HandleAttachRequest LINE 10
- Message Structure:
RRC_DataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. (START_Value)start[20] = '00000000000000000100'B
. ATTACHREQUEST
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)gMMProtocolDiscriminator[4] = '1000'B
. . (MsgType)msgType[8] = '00000001'B
. . MS_NetworkCap_lv
. . . (Length)iel[1] = '02'O
. . . (OctetStringType)value[2] = 'E540'O
. . CiphKeySeqNum
. . . (B1)spare1[1] = '0'B
. . . (KeySeq)keySeq[3] = '000'B
. . AttachType
. . . (B1)pre_for[1] = '0'B
. . . (B3)type[3] = '001'B
. . DRXparamter
. . . (B8)splitPGcycleCode[8] = '00000111'B
. . . (B4)cnDRXcoef[4] = '0000'B
. . . (B1)splitOnCCCH[1] = '0'B
. . . (B3)nonDRXtimer[3] = '010'B
. . MS_Identity_lv
. . . (Length)iel[1] = '05'O
. . . (B4)iDigit1[4] = '1111'B
. . . (B1)oddEvenInd[1] = '0'B
. . . (B3)typeOfId[3] = '100'B
. . . (OctetStringType)otherDigits[4] = '12345678'O
. . RAI_v
. . . (OctetStringType)plmn[3] = '00F110'O
. . . (OctetStringType)lac[2] = '0001'O
. . . (OctetStringType)rac[1] = '05'O
. . MSRadioAccessCap_lv
. . . (Length)iel[1] = '0A'O
. . . (OctetStringType)value[10] = '14F382334C03263CA060'O
. . PTMSI_Signature
. . . (IEI8)iei[8] = '00010111'B
. . . (OctetStringType)value[3] = -
. . GPRS_Timer
. . . (IEI8)iei[8] = '00010110'B
. . . (B3)unit[0] = -
. . . (B5)value[0] = -
. . TMSI_Status
. . . (IEI4)iei[0] = -
. . . (B3)spare3[0] = -
. . . (B1)flag[0] = -
- Constraint:
car_PS_InitDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 03 04 04 00 00 40 08 01 02 e5 40 01 07 02 05 f4 12 34 56 78 00 f1 10 00 01 05 0a 14 f3 82 33 4c 03 26 3c a0 60 17 16

- No.: 1231
- Timestamp: 10:52:20:173_0
- RFN: 2010
- Chip: 27392
- Event: Cancel Timer
- Source: ts_GMM_IdleUpdated:lt_HandleAttachRequest LINE 10
- Message Structure:
no details available
- Constraint:
t_WaitS
- BinaryMessage:

- No.: 1268
- Timestamp: 10:52:20:210_0
- RFN: 2014
- Chip: 15616
- Event: Send
- PCO: Dc
- Message: RRC_DataReq
- Source: ts_GMM_Authentication LINE 2
- Message Structure:
RRC_DataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[-1] = -
. (SapId)sapId[1] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. AUTHENTICATIONANDCIPHERINGREQUEST
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)gMMProtocolDiscriminator[4] = '1000'B
. . (MsgType)msgType[8] = '00010010'B
. . IMEISVRequest
. . . (B1)spare1[1] = '0'B
. . . (B3)value[3] = '000'B
. . CiphAlgorithm
. . . (B1)spare1[1] = '0'B
. . . (B3)algorithm[3] = '001'B
. . AC_ReferenceNumber
. . . (B4)value[4] = '0011'B
. . ForceToStandby
. . . (B1)spare[1] = '0'B
. . . (B3)value[3] = '000'B
. . AuthenticationParamterRAND
. . . (IEI8)iei[8] = '00100001'B
. . . (BitStringType)randValue[128] = '01010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101'B
. . CiphKeySeqNum_tv
. . . (IEI4)iei[4] = '1000'B
. . . (B1)spare1[1] = '0'B
. . . (KeySeq)keySeq[3] = '000'B
. . GMM_AUTN
. . . (IEI8)iei[8] = '00101000'B
. . . (Length)iel[1] = '10'O
. . . (BitStringType)aUTN[128] = '01010110010100010101000001010011010100100101110100000000000000000101010101010100010101110101011001010001010100000101001101010010'B
- Constraint:
ca_PS_DataReq
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 08 12 01 30 21 55 55 55 55 55 55 55 55 55 55 55 55 55 55 55 55 80 28 10 56 51 50 53 52 5d 00 00 55 54 57 56 51 50 53 52

- No.: 1272
- Timestamp: 10:52:20:890_0
- RFN: 2082
- Chip: 18688
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_GMM_Authentication LINE 7
- Message Structure:
RRC_DataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. (START_Value)start[0] = -
. AUTHENTICATIONANDCIPHERINGRESPONSE
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)gMMProtocolDiscriminator[4] = '1000'B
. . (MsgType)msgType[8] = '00010011'B
. . (B4)spare4[4] = '0000'B
. . AC_ReferenceNumber
. . . (B4)value[4] = '0011'B
. . AuthRsp_tv
. . . (IEI8)iei[8] = '00100010'B
. . . (BitStringType)value[32] = '01010101010101000101011101010110'B
. . GMM_MS_Identity
. . AuthRspExt
- Constraint:
car_PS_UplinkDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 08 13 03 22 55 54 57 56

- No.: 1275
- Timestamp: 10:52:20:893_1
- RFN: 2082
- Chip: 30464
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_GMM_Authentication LINE 10
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1312
- Timestamp: 10:52:20:907_0
- RFN: 2084
- Chip: 2816
- Event: Send
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_REQ
- Source: ts_SS_DownloadSecurityKey:lt_DownloadKeyCRLC LINE 1
- Message Structure:
CRLC_SecurityMode_Config_REQ
. (IntegerType)cellId = -1
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity = 1
. . (BitStringType)startValue[20] = "00000000000000000000"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = '01010111010101100101000101010000010100110101001001011101010111000101111101011110010110010101100001011011010110100101010101010100'B
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CRLC_SecurityModeCfgReq
- BinaryMessage:
30 21 02 01 ff 30 1c 0a 01 01 03 04 04 00 00 00 03 11 00 57 56 51 50 53 52 5d 5c 5f 5e 59 58 5b 5a 55 54

- No.: 1313
- Timestamp: 10:52:20:909_0
- RFN: 2084
- Chip: 10496
- Event: Receive
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_CNF
- Source: ts_SS_DownloadSecurityKey:lt_DownloadKeyCRLC LINE 2
- Message Structure:
CRLC_SecurityMode_Config_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1320
- Timestamp: 10:52:20:912_0
- RFN: 2084
- Chip: 22784
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 1
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
. (IntegerType)count_I_LSB_UL = -
. (IntegerType)count_I_LSB_DL = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 00 02 01 00 02 01 00

- No.: 1321
- Timestamp: 10:52:20:914_0
- RFN: 2084
- Chip: 30208
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 2
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 00 02 01 00

- No.: 1322
- Timestamp: 10:52:20:916_0
- RFN: 2084
- Chip: 37120
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 3
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. (IntegerType)count_I_LSB_UL = -
. (IntegerType)count_I_LSB_DL = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 01 02 01 00

- No.: 1323
- Timestamp: 10:52:20:918_0
- RFN: 2085
- Chip: 5888
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 4
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 1324
- Timestamp: 10:52:20:920_0
- RFN: 2085
- Chip: 13312
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 5
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. (IntegerType)count_I_LSB_UL = -
. (IntegerType)count_I_LSB_DL = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 02 02 01 00

- No.: 1325
- Timestamp: 10:52:20:922_0
- RFN: 2085
- Chip: 20480
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 6
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 1326
- Timestamp: 10:52:20:923_0
- RFN: 2085
- Chip: 27648
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 7
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
. (IntegerType)count_I_LSB_UL = -
. (IntegerType)count_I_LSB_DL = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 03 02 01 00

- No.: 1327
- Timestamp: 10:52:20:925_0
- RFN: 2085
- Chip: 34816
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 8
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 1328
- Timestamp: 10:52:20:927_0
- RFN: 2086
- Chip: 3328
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 9
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
. (IntegerType)count_I_LSB_UL = -
. (IntegerType)count_I_LSB_DL = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 04 02 01 00

- No.: 1329
- Timestamp: 10:52:20:929_0
- RFN: 2086
- Chip: 10496
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 10
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 1333
- Timestamp: 10:52:20:932_0
- RFN: 2086
- Chip: 21248
- Event: Send
- PCO: CRLC
- Message: CRLC_Integrity_Activate_REQ
- Source: ts_CRLC_DL_Integrity LINE 1
- Message Structure:
CRLC_Integrity_Activate_REQ
. (IntegerType)cellId = -1
. (CN_DomainIdentity)cn_DomainIdentity = 1
. IntegrityActivationInfo
. . IntegrityProtectionModeInfo
. . . IntegrityProtectionModeCommand
. . . . startIntegrityProtection
. . . . . (BitStringType)integrityProtInitNumber[32] = "00000000000000000000000000000001"
. . . (IntegrityProtectionAlgorithm)integrityProtectionAlgorithm = 0
- Constraint:
ca_CRLC_DL_IntegrityActivateReq
- BinaryMessage:
30 15 02 01 ff 0a 01 01 30 0d 30 30 07 03 05 00 00 00 00 01 0a 01 00

- No.: 1334
- Timestamp: 10:52:20:933_0
- RFN: 2086
- Chip: 27392
- Event: Receive
- PCO: CRLC
- Message: CRLC_Integrity_Activate_CNF
- Source: ts_CRLC_DL_Integrity LINE 2
- Message Structure:
CRLC_Integrity_Activate_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_IntegrityActivateCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1341
- Timestamp: 10:52:20:937_0
- RFN: 2087
- Chip: 4096
- Event: Send
- PCO: CRLC
- Message: CRLC_Integrity_Activate_REQ
- Source: ts_RB2_UL_IntegrityActivate LINE 1
- Message Structure:
CRLC_Integrity_Activate_REQ
. (IntegerType)cellId = -1
. (CN_DomainIdentity)cn_DomainIdentity = 1
. IntegrityActivationInfo
. . IntegrityProtActivationInfoList
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity = 2
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
- Constraint:
ca_CRLC_UL_IntegrityActivateReq
- BinaryMessage:
30 10 02 01 ff 0a 01 01 30 08 30 06 02 01 02 02 01 00

- No.: 1342
- Timestamp: 10:52:20:939_0
- RFN: 2087
- Chip: 11008
- Event: Receive
- PCO: CRLC
- Message: CRLC_Integrity_Activate_CNF
- Source: ts_RB2_UL_IntegrityActivate LINE 2
- Message Structure:
CRLC_Integrity_Activate_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_IntegrityActivateCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1348
- Timestamp: 10:52:20:945_0
- RFN: 2087
- Chip: 33280
- Event: Send
- PCO: AM
- Message: RLC_AM_DATA_REQ
- Source: ts_RRC_Security:lt_SendSecurityModeCommand LINE 7
- Message Structure:
RLC_AM_DATA_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. AmConfirmationRequest
. aM_message
. . DL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00000000000000000000000000000000"
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . DL_DCCH_MessageType
. . . . SecurityModeCommand
. . . . . r3
. . . . . . SecurityModeCommand_r3_IEs
. . . . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . . . SecurityCapability
. . . . . . . . (BitStringType)cipheringAlgorithmCap[16] = '0000000000000011'B
. . . . . . . . (BitStringType)integrityProtectionAlgorithmCap[16] = '0000000000000010'B
. . . . . . . CipheringModeInfo
. . . . . . . IntegrityProtectionModeInfo
. . . . . . . . IntegrityProtectionModeCommand
. . . . . . . . . startIntegrityProtection
. . . . . . . . . . (BitStringType)integrityProtInitNumber[32] = "00000000000000000000000000000001"
. . . . . . . . (IntegrityProtectionAlgorithm)integrityProtectionAlgorithm = 0
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity = 1
. . . . . . . InterRAT_UE_SecurityCapList
. . . . . . laterNonCriticalExtensions
- Constraint:
cas_RRC_SecModeCmd
- BinaryMessage:
30 17 02 01 ff 02 01 02 05 00 80 00 00 00 04 04 00 01 80 01 40 00 00 00 30

- No.: 1354
- Timestamp: 10:52:21:079_0
- RFN: 2101
- Chip: 13312
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_IND
- Source: ts_RRC_Security:lt_StartSecurity_UE LINE 8
- Message Structure:
RLC_AM_DATA_IND
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. IntegrityResult
. . (IntegrityStatus)integrityUsed = 0
. aM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "10000001100000001110110111011101"
. . . . (IntegerType)rrc_MessageSequenceNumber = 1
. . . UL_DCCH_MessageType
. . . . SecurityModeComplete
. . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . IntegrityProtActivationInfo
. . . . . . RRC_MessageSequenceNumberList
. . . . . . . (IntegerType)_elem = 0
. . . . . . . (IntegerType)_elem = 0
. . . . . . . (IntegerType)_elem = 0
. . . . . . . (IntegerType)_elem = 0
. . . . . . . (IntegerType)_elem = 0
. . . . . laterNonCriticalExtensions
. . . . . . (BitStringType)securityModeComplete_r3_add_ext = 0
. . . . . . nonCriticalExtensions
- Constraint:
car_RRC_SecModeCmpl
- BinaryMessage:
30 12 02 01 ff 02 01 02 0a 01 00 c0 c0 76 ee 8d 21 00 00 00

- No.: 1355
- Timestamp: 10:52:21:080_0
- RFN: 2101
- Chip: 17408
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_Security:lt_StartSecurity_UE LINE 8
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1357
- Timestamp: 10:52:21:084_0
- RFN: 2101
- Chip: 32768
- Event: Send
- PCO: CRLC
- Message: CRLC_Integrity_Activate_REQ
- Source: ts_CRLC_UL_Integrity LINE 1
- Message Structure:
CRLC_Integrity_Activate_REQ
. (IntegerType)cellId = -1
. (CN_DomainIdentity)cn_DomainIdentity = 1
. IntegrityActivationInfo
. . IntegrityProtActivationInfoList
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity = 0
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity = 1
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity = 3
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity = 4
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
- Constraint:
ca_CRLC_UL_IntegrityActivateReq
- BinaryMessage:
30 28 02 01 ff 0a 01 01 30 20 30 06 02 01 00 02 01 00 30 06 02 01 01 02 01 00 30 06 02 01 03 02 01 00 30 06 02 01 04 02 01 00

- No.: 1358
- Timestamp: 10:52:21:086_0
- RFN: 2102
- Chip: 1280
- Event: Receive
- PCO: CRLC
- Message: CRLC_Integrity_Activate_CNF
- Source: ts_CRLC_UL_Integrity LINE 2
- Message Structure:
CRLC_Integrity_Activate_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_IntegrityActivateCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1368
- Timestamp: 10:52:21:111_0
- RFN: 2104
- Chip: 19200
- Event: Send
- PCO: Dc
- Message: RRC_DataReq
- Source: ts_GMM_IdleUpdated:lt_AttachAccept LINE 12
- Message Structure:
RRC_DataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[-1] = -
. (SapId)sapId[1] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. ATTACHACCEPT
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)gMMProtocolDiscriminator[4] = '1000'B
. . (MsgType)msgType[8] = '00000010'B
. . ForceToStandby
. . . (B1)spare[1] = '0'B
. . . (B3)value[3] = '000'B
. . AttachResult
. . . (B1)spare[1] = '0'B
. . . (B3)result[3] = '001'B
. . GPRS_Timer_v
. . . (B3)unit[3] = '111'B
. . . (B5)value[5] = '00000'B
. . (B4)spare[4] = '0000'B
. . RadioPriority_v
. . . (B1)spare[1] = '0'B
. . . (B3)value[3] = '100'B
. . RAI_v
. . . (OctetStringType)plmn[3] = '00F110'O
. . . (OctetStringType)lac[2] = '0001'O
. . . (OctetStringType)rac[1] = '05'O
. . PTMSI_Signature
. . . (IEI8)iei[8] = '00011001'B
. . . (OctetStringType)value[3] = 'AB1234'O
. . GPRS_Timer
. . GMM_MS_IdentityPTMSI
. . . (IEI8)iei[8] = '00011000'B
. . . (Length)iel[1] = '05'O
. . . (B4)iDigit1[4] = '1111'B
. . . (B1)oddEvenInd[1] = '0'B
. . . (B3)typeOfId[3] = '100'B
. . . (OctetStringType)otherDigits[-1] = '12345678'O
. . GMM_MS_Identity
. . GMM_Cause
. . GPRS_Timer
. . CellNotification
. . PLMN_List
- Constraint:
ca_PS_DataReq
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 08 02 01 e0 04 00 f1 10 00 01 05 19 ab 12 34 18 05 f4 12 34 56 78

- No.: 1372
- Timestamp: 10:52:21:258_0
- RFN: 2119
- Chip: 5632
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_GMM_IdleUpdated:lt_AttachAccept LINE 13
- Message Structure:
RRC_DataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. (START_Value)start[0] = -
. ATTACHCOMPLETE
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)gMMProtocolDiscriminator[4] = '1000'B
. . (MsgType)msgType[8] = '00000011'B
- Constraint:
car_PS_UplinkDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 08 03

- No.: 1383
- Timestamp: 10:52:21:261_2
- RFN: 2119
- Chip: 19200
- Event: Start Timer
- Source: ts_RRC_Delay LINE 1
- Message Structure:
no details available
- Constraint:
t_Dly (1000 Ms)
- BinaryMessage:

- No.: 1387
- Timestamp: 10:52:22:263_0
- RFN: 2219
- Chip: 27392
- Event: Timeout
- Source: ts_RRC_Delay LINE 2
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 1392
- Timestamp: 10:52:22:268_0
- RFN: 2220
- Chip: 9472
- Event: Send
- PCO: UM
- Message: RLC_UM_DATA_REQ
- Source: ts_RRC_ConnRel:lt_Send_RRC_ConnectionRelease LINE 3
- Message Structure:
RLC_UM_DATA_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. uM_message
. . DL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00000000000000000000000000000000"
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . DL_DCCH_MessageType
. . . . RRCConnectionRelease
. . . . . r3
. . . . . . RRCConnectionRelease_r3_IEs
. . . . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . . . (IntegerType)n_308 = 1
. . . . . . . (ReleaseCause)releaseCause = 0
. . . . . . . Rplmn_Information
. . . . . . laterNonCriticalExtensions
. (BooleanType)specialLI = FALSE
- Constraint:
cas_RRC_ConnRelDCCH
- BinaryMessage:
30 10 02 01 ff 02 01 01 80 00 00 00 03 c8 00 01 01 00

- No.: 1396
- Timestamp: 10:52:22:398_0
- RFN: 2233
- Chip: 8960
- Event: Receive
- PCO: UM
- Message: RLC_UM_DATA_IND
- Source: ts_RRC_ConnRel:lt_Send_RRC_ConnectionRelease LINE 4
- Message Structure:
RLC_UM_DATA_IND
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. IntegrityResult
. uM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "10101101101011101001000000111001"
. . . . (IntegerType)rrc_MessageSequenceNumber = 1
. . . UL_DCCH_MessageType
. . . . RRCConnectionReleaseComplete
. . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . FailureCauseWithProtErr
. . . . . laterNonCriticalExtensions
. . . . . . (BitStringType)rrcConnectionReleaseComplete_r3_add_ext = 0
. . . . . . nonCriticalExtensions
- Constraint:
car_RRC_ConnRelCmplUM
- BinaryMessage:
30 0c 02 01 ff 02 01 01 d6 d7 48 1c 8c 40

- No.: 1397
- Timestamp: 10:52:22:399_0
- RFN: 2233
- Chip: 12288
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ConnRel:lt_Send_RRC_ConnectionRelease LINE 4
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1400
- Timestamp: 10:52:22:400_2
- RFN: 2233
- Chip: 17920
- Event: Start Timer
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 1
- Message Structure:
no details available
- Constraint:
t_Dly (5000 Ms)
- BinaryMessage:

- No.: 1404
- Timestamp: 10:52:22:548_0
- RFN: 2248
- Chip: 8192
- Event: Receive
- PCO: UM
- Message: RLC_UM_DATA_IND
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 4
- Message Structure:
RLC_UM_DATA_IND
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. IntegrityResult
. uM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00011100010101000111110101101001"
. . . . (IntegerType)rrc_MessageSequenceNumber = 2
. . . UL_DCCH_MessageType
. . . . RRCConnectionReleaseComplete
. . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . FailureCauseWithProtErr
. . . . . laterNonCriticalExtensions
. . . . . . (BitStringType)rrcConnectionReleaseComplete_r3_add_ext = 0
. . . . . . nonCriticalExtensions
- Constraint:
car_RRC_ConnRelCmplUM
- BinaryMessage:
30 0c 02 01 ff 02 01 01 8e 2a 3e b4 94 40

- No.: 1405
- Timestamp: 10:52:22:549_0
- RFN: 2248
- Chip: 12288
- Event: Cancel Timer
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 4
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 1406
- Timestamp: 10:52:22:550_0
- RFN: 2248
- Chip: 13312
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 4
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1412
- Timestamp: 10:52:22:553_0
- RFN: 2248
- Chip: 26880
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 01 0a 01 00 05 00

- No.: 1416
- Timestamp: 10:52:22:566_0
- RFN: 2249
- Chip: 36864
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 1419
- Timestamp: 10:52:22:568_0
- RFN: 2250
- Chip: 9216
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 02 0a 01 00 05 00

- No.: 1423
- Timestamp: 10:52:22:578_0
- RFN: 2251
- Chip: 6656
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 1426
- Timestamp: 10:52:22:581_0
- RFN: 2251
- Chip: 18432
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 03 0a 01 00 05 00

- No.: 1430
- Timestamp: 10:52:22:588_0
- RFN: 2252
- Chip: 9216
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 1433
- Timestamp: 10:52:22:591_0
- RFN: 2252
- Chip: 19968
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 04 0a 01 00 05 00

- No.: 1437
- Timestamp: 10:52:22:599_0
- RFN: 2253
- Chip: 11520
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 1440
- Timestamp: 10:52:22:606_0
- RFN: 2254
- Chip: 1536
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 136
. . . . . UL_RLC_Mode
. . . . . . UL_UM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (NoExplicitDiscard)timerBasedNoExplicit = 9
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = 1
. . . . (IntegerType)dLlogicalChannelIdentity = 1
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_UM_Info
- BinaryMessage:
30 22 02 01 ff 02 01 01 0a 01 00 30 17 30 0d 05 00 30 09 02 02 00 88 30 03 0a 01 09 30 06 02 01 01 02 01 01

- No.: 1444
- Timestamp: 10:52:22:617_0
- RFN: 2255
- Chip: 5888
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 1445
- Timestamp: 10:52:22:626_0
- RFN: 2255
- Chip: 37888
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 3
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . (TimerEPC)timerEPC = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . (TimerRST)timerRST = 9
. . . . . . . (MaxRST)max_RST = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = 2
. . . . (IntegerType)dLlogicalChannelIdentity = 2
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 02 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 27 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 02 02 01 02

- No.: 1449
- Timestamp: 10:52:22:643_0
- RFN: 2257
- Chip: 27904
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 4
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 1450
- Timestamp: 10:52:22:652_0
- RFN: 2258
- Chip: 23040
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 5
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . (TimerEPC)timerEPC = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . (TimerRST)timerRST = 9
. . . . . . . (MaxRST)max_RST = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = 3
. . . . (IntegerType)dLlogicalChannelIdentity = 3
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 03 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 27 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 03 02 01 03

- No.: 1454
- Timestamp: 10:52:22:668_0
- RFN: 2260
- Chip: 7168
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 6
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 1455
- Timestamp: 10:52:22:676_0
- RFN: 2261
- Chip: 2560
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 7
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . (TimerEPC)timerEPC = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . (TimerRST)timerRST = 9
. . . . . . . (MaxRST)max_RST = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = 4
. . . . (IntegerType)dLlogicalChannelIdentity = 4
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 04 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 27 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 04 02 01 04

- No.: 1459
- Timestamp: 10:52:22:694_0
- RFN: 2262
- Chip: 31744
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 8
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 1501
- Timestamp: 10:52:22:728_0
- RFN: 2266
- Chip: 8192
- Event: Start Timer
- Source: ts_RRC_Delay LINE 1
- Message Structure:
no details available
- Constraint:
t_Dly (5000 Ms)
- BinaryMessage:

- No.: 1503
- Timestamp: 10:52:22:730_0
- RFN: 2266
- Chip: 18688
- Event: Receive
- PCO: CPHY
- Message: CPHY_Out_of_Sync_IND
- Source: RRC_Def1 LINE 15
- Message Structure:
CPHY_Out_of_Sync_IND
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_OutOfSyncInd
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 1504
- Timestamp: 10:52:22:731_0
- RFN: 2266
- Chip: 20480
- Event: Cancel Timer
- Source: RRC_Def1 LINE 15
- Message Structure:
no details available
- Constraint:
t_T312
- BinaryMessage:

- No.: 1505
- Timestamp: 10:52:22:731_1
- RFN: 2266
- Chip: 22528
- Event: Default
- Source: RRC_Def1 LINE 0
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1506
- Timestamp: 10:52:22:732_0
- RFN: 2266
- Chip: 23296
- Event: Default
- Source: ts_RRC_Delay LINE 2
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1511
- Timestamp: 10:52:27:716_0
- RFN: 2765
- Chip: 2048
- Event: Timeout
- Source: ts_RRC_Delay LINE 2
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 1524
- Timestamp: 10:52:27:735_0
- RFN: 2766
- Chip: 36608
- Event: Send
- PCO: CMAC
- Message: CMAC_PAGING_Config_REQ
- Source: ts_CMAC_Pag1_Cfg LINE 4
- Message Structure:
CMAC_PAGING_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 5
. (RatType)ratType = 0
. CmacPagingConfigReq
. . pI_BitMapInfo
. . . (BitStringType)e18[18] = '010000000000000000'B
. . (IntegerType)dRX_CycleLength = 7
. . IMSI_GSM_MAP
. . . (IntegerType)_elem = 0
. . . (IntegerType)_elem = 0
. . . (IntegerType)_elem = 1
. . . (IntegerType)_elem = 0
. . . (IntegerType)_elem = 1
. . . (IntegerType)_elem = 0
. . . (IntegerType)_elem = 1
. . . (IntegerType)_elem = 2
. . . (IntegerType)_elem = 3
. . . (IntegerType)_elem = 4
. . . (IntegerType)_elem = 5
. . . (IntegerType)_elem = 6
. . . (IntegerType)_elem = 0
. . . (IntegerType)_elem = 6
. . . (IntegerType)_elem = 3
. . (BooleanType)t_pich_T_sccpch = FALSE
- Constraint:
ca_CMAC_PagingCfgReq
- BinaryMessage:
30 46 02 01 00 02 01 05 0a 01 00 30 3b 03 04 06 40 00 00 02 01 07 30 2d 02 01 00 02 01 00 02 01 01 02 01 00 02 01 01 02 01 00 02 01 01 02 01 02 02 01 03 02 01 04 02 01 05 02 01 06 02 01 00 02 01 06 02 01 03 01 01 00

- No.: 1528
- Timestamp: 10:52:27:743_0
- RFN: 2767
- Chip: 30208
- Event: Receive
- PCO: CMAC
- Message: CMAC_PAGING_Config_CNF
- Source: ts_CMAC_Pag1_Cfg LINE 5
- Message Structure:
CMAC_PAGING_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 5
- Constraint:
ca_CMAC_PagingCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 05

- No.: 1530
- Timestamp: 10:52:27:772_0
- RFN: 2770
- Chip: 26368
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_RRC_ConnEst_DCH_MT_PTMSI LINE 5
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -2
. tM_message
. . PCCH_Message
. . . PCCH_MessageType
. . . . PagingType1
. . . . . PagingRecordList
. . . . . . PagingRecord
. . . . . . . cn_Identity
. . . . . . . . (PagingCause)pagingCause = 2
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = 1
. . . . . . . . CN_PagedUE_Identity
. . . . . . . . . (BitStringType)p_TMSI_GSM_MAP[32] = "00010010001101000101011001111000"
. . . . . BCCH_ModificationInfo
. . . . . laterNonCriticalExtensions
- Constraint:
cas_PagingType1
- BinaryMessage:
30 0c 02 01 00 02 01 fe 40 54 24 68 ac f0

- No.: 1534
- Timestamp: 10:52:29:106_0
- RFN: 2904
- Chip: 256
- Event: Receive
- PCO: TM
- Message: RLC_TR_DATA_IND
- Source: ts_RRC_ConnEst_DCH_MT_PTMSI LINE 6
- Message Structure:
RLC_TR_DATA_IND
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
. tM_message
. . UL_CCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode = 0
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . UL_CCCH_MessageType
. . . . RRCConnectionRequest
. . . . . InitialUE_Identity
. . . . . . TMSI_and_LAI_GSM_MAP
. . . . . . . (BitStringType)tmsi[32] = "00010010001101000101011001111000"
. . . . . . . LAI
. . . . . . . . PLMN_Identity
. . . . . . . . . MCC
. . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . (IntegerType)_elem = 1
. . . . . . . . . MNC
. . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . (IntegerType)_elem = 1
. . . . . . . . (BitStringType)lac[16] = '0000000000000001'B
. . . . . (EstablishmentCause)establishmentCause = 7
. . . . . (ProtocolErrorIndicator)protocolErrorIndicator = 0
. . . . . MeasuredResultsOnRACH
. . . . . . currentCell
. . . . . . . modeSpecificInfo
. . . . . . . . fdd
. . . . . . . . . measurementQuantity
. . . . . . . . . . (IntegerType)cpich_Ec_N0 = 0
. . . . . v3d0NonCriticalExtensions
. . . . . . RRCConnectionRequest_v3d0ext_IEs
. . . . . . . (BitStringType)uESpecificBehaviourInformation1idle = 0
. . . . . . nonCriticalExtensions
- Constraint:
car_RRC_ConnReq
- BinaryMessage:
30 11 02 01 00 02 01 00 21 12 34 56 78 00 10 08 00 09 c0

- No.: 1535
- Timestamp: 10:52:29:170_0
- RFN: 2910
- Chip: 16640
- Event: Send
- PCO: UM
- Message: RLC_UM_DATA_REQ
- Source: ts_RRC_ConnEst_DCH_MT_PTMSI LINE 7
- Message Structure:
RLC_UM_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
. uM_message
. . DL_CCCH_Message
. . . IntegrityCheckInfo
. . . DL_CCCH_MessageType
. . . . RRCConnectionSetup
. . . . . r3
. . . . . . RRCConnectionSetup_r3_IEs
. . . . . . . InitialUE_Identity
. . . . . . . . TMSI_and_LAI_GSM_MAP
. . . . . . . . . (BitStringType)tmsi[32] = "00010010001101000101011001111000"
. . . . . . . . . LAI
. . . . . . . . . . PLMN_Identity
. . . . . . . . . . . MCC
. . . . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . . . (IntegerType)_elem = 1
. . . . . . . . . . . MNC
. . . . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . . . (IntegerType)_elem = 1
. . . . . . . . . . (BitStringType)lac[16] = '0000000000000001'B
. . . . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . . . (IntegerType)activationTime = -
. . . . . . . U_RNTI
. . . . . . . . (BitStringType)srnc_Identity[12] = "000000000001"
. . . . . . . . (BitStringType)s_RNTI[20] = "00000000000000000001"
. . . . . . . (BitStringType)new_c_RNTI[16] = -
. . . . . . . (RRC_StateIndicator)rrc_StateIndicator = 0
. . . . . . . (IntegerType)utran_DRX_CycleLengthCoeff = 9
. . . . . . . CapabilityUpdateRequirement
. . . . . . . . (BooleanType)ue_RadioCapabilityFDDUpdateRequirement = TRUE
. . . . . . . . (BooleanType)ue_RadioCapabilityTDDUpdateRequirement = FALSE
. . . . . . . . SystemSpecificCapUpdateReqList
. . . . . . . . . (SystemSpecificCapUpdateReq)_elem = 0
. . . . . . . SRB_InformationSetupList2
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_UM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 1
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 1
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . . . . . . . (TimerRST)timerRST = 9
. . . . . . . . . . . . . (MaxRST)max_RST = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 2
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 2
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . . . . . . . (TimerRST)timerRST = 9
. . . . . . . . . . . . . (MaxRST)max_RST = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 3
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 3
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . . . . . . . (TimerRST)timerRST = 9
. . . . . . . . . . . . . (MaxRST)max_RST = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 4
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 4
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . UL_CommonTransChInfo
. . . . . . . . TFC_Subset
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . TFCS
. . . . . . . . . . . ExplicitTFCS_Configuration
. . . . . . . . . . . . TFCS_ReconfAdd
. . . . . . . . . . . . . ctfcSize
. . . . . . . . . . . . . . ctfc2Bit
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . . . . . . . (IntegerType)ctfc2 = 0
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . . . . . . . (IntegerType)ctfc2 = 1
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 11
. . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . UL_AddReconfTransChInfoList
. . . . . . . . UL_AddReconfTransChInformation
. . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType = 0
. . . . . . . . . (IntegerType)transportChannelIdentity = 5
. . . . . . . . . TransportFormatSet
. . . . . . . . . . DedicatedTransChTFS
. . . . . . . . . . . tti
. . . . . . . . . . . . DedicatedDynamicTF_InfoList
. . . . . . . . . . . . . DedicatedDynamicTF_Info
. . . . . . . . . . . . . . rlc_Size
. . . . . . . . . . . . . . . BitModeRLC_SizeInfo
. . . . . . . . . . . . . . . . sizeType2
. . . . . . . . . . . . . . . . . (IntegerType)part1 = 2
. . . . . . . . . . . . . . . . . (IntegerType)part2 = -
. . . . . . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . LogicalChannelList
. . . . . . . . . . . SemistaticTF_Information
. . . . . . . . . . . . ChannelCodingType
. . . . . . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . . . . . (IntegerType)rateMatchingAttribute = 192
. . . . . . . . . . . . (CRC_Size)crc_Size = 3
. . . . . . . DL_CommonTransChInfo
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . dl_Parameters
. . . . . . . DL_AddReconfTransChInfoList
. . . . . . . . DL_AddReconfTransChInformation
. . . . . . . . . (DL_TrCH_Type)dl_TransportChannelType = 0
. . . . . . . . . (IntegerType)dl_transportChannelIdentity = 10
. . . . . . . . . tfs_SignallingMode
. . . . . . . . . . UL_TransportChannelIdentity
. . . . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType = 0
. . . . . . . . . . . (IntegerType)ul_TransportChannelIdentity = 5
. . . . . . . . . QualityTarget
. . . . . . . . . . (IntegerType)bler_QualityValue = -20
. . . . . . . . . TM_SignallingInfo
. . . . . . . FrequencyInfo
. . . . . . . (IntegerType)maxAllowedUL_TX_Power = -
. . . . . . . UL_ChannelRequirement
. . . . . . . . UL_DPCH_Info
. . . . . . . . . UL_DPCH_PowerControlInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (IntegerType)dpcch_PowerOffset = -40
. . . . . . . . . . . (IntegerType)pc_Preamble = 1
. . . . . . . . . . . (IntegerType)sRB_delay = 7
. . . . . . . . . . . PowerControlAlgorithm
. . . . . . . . . . . . (IntegerType)algorithm1 = 1
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (ScramblingCodeType)scramblingCodeType = 1
. . . . . . . . . . . (IntegerType)scramblingCode = 0
. . . . . . . . . . . (IntegerType)numberOfDPDCH = -
. . . . . . . . . . . (SpreadingFactor)spreadingFactor = 4
. . . . . . . . . . . (BooleanType)tfci_Existence = TRUE
. . . . . . . . . . . (IntegerType)numberOfFBI_Bits = -
. . . . . . . . . . . (PuncturingLimit)puncturingLimit = 15
. . . . . . . DL_CommonInformation
. . . . . . . . DL_DPCH_InfoCommon
. . . . . . . . . cfnHandling
. . . . . . . . . . initialise
. . . . . . . . . . . (IntegerType)cfntargetsfnframeoffset = -
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . DL_DPCH_PowerControlInfo
. . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . (DPC_Mode)dpc_Mode = 0
. . . . . . . . . . . (IntegerType)powerOffsetPilot_pdpdch = 0
. . . . . . . . . . . Dl_rate_matching_restriction
. . . . . . . . . . . SF512_AndPilot
. . . . . . . . . . . . (PilotBits128)sfd128 = 0
. . . . . . . . . . . (PositionFixedOrFlexible)positionFixedOrFlexible = 0
. . . . . . . . . . . (BooleanType)tfci_Existence = FALSE
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . (IntegerType)defaultDPCH_OffsetValue = 0
. . . . . . . . . . DPCH_CompressedModeInfo
. . . . . . . . . . (TX_DiversityMode)tx_DiversityMode = 0
. . . . . . . . . . SSDT_Information
. . . . . . . DL_InformationPerRL_List
. . . . . . . . DL_InformationPerRL
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . PrimaryCPICH_Info
. . . . . . . . . . . . (IntegerType)primaryScramblingCode = 100
. . . . . . . . . . . PDSCH_SHO_DCH_Info
. . . . . . . . . . . PDSCH_CodeMapping
. . . . . . . . . DL_DPCH_InfoPerRL
. . . . . . . . . . fdd
. . . . . . . . . . . (PCPICH_UsageForChannelEst)pCPICH_UsageForChannelEst = 0
. . . . . . . . . . . (IntegerType)dpch_FrameOffset = 0
. . . . . . . . . . . SecondaryCPICH_Info
. . . . . . . . . . . DL_ChannelisationCodeList
. . . . . . . . . . . . DL_ChannelisationCode
. . . . . . . . . . . . . (IntegerType)secondaryScramblingCode = 1
. . . . . . . . . . . . . SF512_AndCodeNumber
. . . . . . . . . . . . . . (IntegerType)sf128 = 0
. . . . . . . . . . . . . (ScramblingCodeChange)scramblingCodeChange = 1
. . . . . . . . . . . (IntegerType)tpc_CombinationIndex = 0
. . . . . . . . . . . (SSDT_CellIdentity)ssdt_CellIdentity = -
. . . . . . . . . . . (ClosedLoopTimingAdjMode)closedLoopTimingAdjMode = -
. . . . . . . . . SCCPCH_InfoForFACH
. . . . . . laterNonCriticalExtensions
. (BooleanType)specialLI = TRUE
- Constraint:
cas_RRC_ConnSetup
- BinaryMessage:
30 78 02 01 00 02 01 00 30 e7 22 46 8a cf 00 02 01 00 01 00 04 00 00 4d 82 69 3a 10 10 89 0d 42 00 02 81 9e 8e 46 c9 ce 7c 9c 4e 74 20 a5 12 3a 8c 00 15 13 3d 1c 8d 93 9c f9 38 9c e8 42 52 24 b5 28 00 4a 46 7a 39 1b 27 39 f2 71 39 d0 86 b4 49 ea 70 00 d4 c8 00 06 25 2b f0 02 00 08 82 23 bf 66 08 98 95 a5 47 a2 00 00 01 3f 90 0a 14 00 02 06 40 00 0c 28 08 01 01 ff

- No.: 1543
- Timestamp: 10:52:29:212_1
- RFN: 2914
- Chip: 23808
- Event: Start Timer
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 3
- Message Structure:
no details available
- Constraint:
t_WaitMS (13500 Ms)
- BinaryMessage:

- No.: 1548
- Timestamp: 10:52:29:444_0
- RFN: 2937
- Chip: 32000
- Event: Receive
- PCO: CPHY
- Message: CPHY_Sync_IND
- Source: RRC_Def1 LINE 13
- Message Structure:
CPHY_Sync_IND
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_SyncInd
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 1549
- Timestamp: 10:52:29:445_0
- RFN: 2937
- Chip: 34048
- Event: Cancel Timer
- Source: RRC_Def1 LINE 13
- Message Structure:
no details available
- Constraint:
t_T312
- BinaryMessage:

- No.: 1550
- Timestamp: 10:52:29:445_1
- RFN: 2937
- Chip: 35584
- Event: Default
- Source: RRC_Def1 LINE 0
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1551
- Timestamp: 10:52:29:446_0
- RFN: 2937
- Chip: 36864
- Event: Default
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1556
- Timestamp: 10:52:29:559_0
- RFN: 2949
- Chip: 11520
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_IND
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
RLC_AM_DATA_IND
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. IntegrityResult
. . (IntegrityStatus)integrityUsed = 0
. aM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode = 0
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . UL_DCCH_MessageType
. . . . RRCConnectionSetupComplete
. . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . STARTList
. . . . . . STARTSingle
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity = 1
. . . . . . . (BitStringType)start_Value[20] = "00000000000000000010"
. . . . . . STARTSingle
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity = 0
. . . . . . . (BitStringType)start_Value[20] = "00000000000000000010"
. . . . . UE_RadioAccessCapability
. . . . . . (AccessStratumReleaseIndicator)accessStratumReleaseIndicator = 0
. . . . . . PDCP_Capability
. . . . . . . (BooleanType)losslessSRNS_RelocationSupport = FALSE
. . . . . . . supportForRfc2507
. . . . . . RLC_Capability
. . . . . . . (TotalRLC_AM_BufferSize)totalRLC_AM_BufferSize = 2
. . . . . . . (MaximumRLC_WindowSize)maximumRLC_WindowSize = 0
. . . . . . . (MaximumAM_EntityNumberRLC_Cap)maximumAM_EntityNumber = 3
. . . . . . TransportChannelCapability
. . . . . . . DL_TransChCapability
. . . . . . . . (MaxNoBits)maxNoBitsReceived = 4
. . . . . . . . (MaxNoBits)maxConvCodeBitsReceived = 1
. . . . . . . . TurboSupport
. . . . . . . . . (MaxNoBits)supported = 4
. . . . . . . . (MaxSimultaneousTransChsDL)maxSimultaneousTransChs = 1
. . . . . . . . (IntegerType)maxSimultaneousCCTrCH_Count = 1
. . . . . . . . (MaxTransportBlocksDL)maxReceivedTransportBlocks = 2
. . . . . . . . (MaxNumberOfTFC_DL)maxNumberOfTFC = 4
. . . . . . . . (MaxNumberOfTF)maxNumberOfTF = 1
. . . . . . . UL_TransChCapability
. . . . . . . . (MaxNoBits)maxNoBitsTransmitted = 3
. . . . . . . . (MaxNoBits)maxConvCodeBitsTransmitted = 1
. . . . . . . . TurboSupport
. . . . . . . . . (MaxNoBits)supported = 3
. . . . . . . . (MaxSimultaneousTransChsUL)maxSimultaneousTransChs = 2
. . . . . . . . modeSpecificInfo
. . . . . . . . (MaxTransportBlocksUL)maxTransmittedBlocks = 2
. . . . . . . . (MaxNumberOfTFC_UL)maxNumberOfTFC = 3
. . . . . . . . (MaxNumberOfTF)maxNumberOfTF = 0
. . . . . . RF_Capability
. . . . . . . fddRF_Capability
. . . . . . . . (IntegerType)ue_PowerClass = 4
. . . . . . . . (TxRxFrequencySeparation)txRxFrequencySeparation = 0
. . . . . . . tddRF_Capability
. . . . . . . . (IntegerType)ue_PowerClass = 0
. . . . . . . . (RadioFrequencyBandTDDList)radioFrequencyTDDBandList = 0
. . . . . . . . (ChipRateCapability)chipRateCapability = 0
. . . . . . PhysicalChannelCapability
. . . . . . . fddPhysChCapability
. . . . . . . . DL_PhysChCapabilityFDD
. . . . . . . . . (IntegerType)maxNoDPCH_PDSCH_Codes = 3
. . . . . . . . . (MaxNoPhysChBitsReceived)maxNoPhysChBitsReceived = 6
. . . . . . . . . (BooleanType)supportForSF_512 = FALSE
. . . . . . . . . (BooleanType)supportOfPDSCH = FALSE
. . . . . . . . . SimultaneousSCCPCH_DPCH_Reception
. . . . . . . . UL_PhysChCapabilityFDD
. . . . . . . . . (MaxNoDPDCH_BitsTransmitted)maxNoDPDCH_BitsTransmitted = 2
. . . . . . . . . (BooleanType)supportOfPCPCH = FALSE
. . . . . . . tddPhysChCapability
. . . . . . . . DL_PhysChCapabilityTDD
. . . . . . . . . (IntegerType)maxTS_PerFrame = 0
. . . . . . . . . (IntegerType)maxPhysChPerFrame = 0
. . . . . . . . . (MinimumSF_DL)minimumSF = 0
. . . . . . . . . (BooleanType)supportOfPDSCH = FALSE
. . . . . . . . . (IntegerType)maxPhysChPerTS = 0
. . . . . . . . UL_PhysChCapabilityTDD
. . . . . . . . . (IntegerType)maxTS_PerFrame = 0
. . . . . . . . . (MaxPhysChPerTimeslot)maxPhysChPerTimeslot = 0
. . . . . . . . . (MinimumSF_UL)minimumSF = 0
. . . . . . . . . (BooleanType)supportOfPUSCH = FALSE
. . . . . . UE_MultiModeRAT_Capability
. . . . . . . MultiRAT_Capability
. . . . . . . . (BooleanType)supportOfGSM = TRUE
. . . . . . . . (BooleanType)supportOfMulticarrier = FALSE
. . . . . . . (MultiModeCapability)multiModeCapability = 1
. . . . . . SecurityCapability
. . . . . . . (BitStringType)cipheringAlgorithmCap[16] = '0000000000000011'B
. . . . . . . (BitStringType)integrityProtectionAlgorithmCap[16] = '0000000000000010'B
. . . . . . UE_Positioning_Capability
. . . . . . . (BooleanType)standaloneLocMethodsSupported = FALSE
. . . . . . . (BooleanType)ue_BasedOTDOA_Supported = FALSE
. . . . . . . (NetworkAssistedGPS_Supported)networkAssistedGPS_Supported = 3
. . . . . . . (BooleanType)supportForUE_GPS_TimingOfCellFrames = FALSE
. . . . . . . (BooleanType)supportForIPDL = FALSE
. . . . . . MeasurementCapability
. . . . . . . CompressedModeMeasCapability
. . . . . . . . (BooleanType)fdd_Measurements = TRUE
. . . . . . . . (BooleanType)tdd_Measurements = FALSE
. . . . . . . . GSM_Measurements
. . . . . . . . . (BooleanType)gsm900 = TRUE
. . . . . . . . . (BooleanType)dcs1800 = TRUE
. . . . . . . . . (BooleanType)gsm1900 = FALSE
. . . . . . . . (BooleanType)multiCarrierMeasurements = FALSE
. . . . . . . CompressedModeMeasCapability
. . . . . . . . (BooleanType)fdd_Measurements = TRUE
. . . . . . . . (BooleanType)tdd_Measurements = FALSE
. . . . . . . . GSM_Measurements
. . . . . . . . . (BooleanType)gsm900 = TRUE
. . . . . . . . . (BooleanType)dcs1800 = TRUE
. . . . . . . . . (BooleanType)gsm1900 = FALSE
. . . . . . . . (BooleanType)multiCarrierMeasurements = FALSE
. . . . . v370NonCriticalExtensions
. . . . . . RRCConnectionSetupComplete_v370ext
. . . . . . . UE_RadioAccessCapability_v370ext
. . . . . . v380NonCriticalExtensions
. . . . . . . RRCConnectionSetupComplete_v380ext_IEs
. . . . . . . . UE_RadioAccessCapability_v380ext
. . . . . . . . . UE_PositioningCapabilityExt_v380
. . . . . . . . . . (BooleanType)rx_tx_TimeDifferenceType2Capable = FALSE
. . . . . . . . DL_PhysChCapabilityFDD_v380ext
. . . . . . . . . (SupportOfDedicatedPilotsForChEstimation)supportOfDedicatedPilotsForChEstimation = 0
. . . . . . . v3a0NonCriticalExtensions
. . . . . . . . RRCConnectionSetupComplete_v3a0ext_IEs
. . . . . . . . . UE_RadioAccessCapability_v3a0ext
. . . . . . . . . . UE_PositioningCapabilityExt_v3a0
. . . . . . . . . . . (UE_PositioningCapabilityExt_v3a0_list_0)validity_CellPCH_UraPCH = 0
. . . . . . . . laterNonCriticalExtensions
. . . . . . . . . (BitStringType)rrcConnectionSetupComplete_r3_add_ext = 0
. . . . . . . . . nonCriticalExtensions
- Constraint:
car_RRC_ConnSetupCmpl
- BinaryMessage:
30 27 02 01 ff 02 01 02 0a 05 01 00 00 00 00 4a 0c 00 00 80 00 05 11 a0 d1 04 84 c6 68 46 2c 93 02 48 00 18 00 11 8f 8f 80

- No.: 1557
- Timestamp: 10:52:29:569_0
- RFN: 2950
- Chip: 13056
- Event: Cancel Timer
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
t_WaitMS
- BinaryMessage:

- No.: 1558
- Timestamp: 10:52:29:569_1
- RFN: 2950
- Chip: 14080
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1572
- Timestamp: 10:52:29:576_0
- RFN: 2951
- Chip: 768
- Event: Send
- PCO: CMAC
- Message: CMAC_SecurityMode_Config_REQ
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 1
- Message Structure:
CMAC_SecurityMode_Config_REQ
. (IntegerType)cellId = 0
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity = 1
. . (BitStringType)startValue[20] = "00000000000000000010"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = -
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CMAC_SecurityModeCfgReq
- BinaryMessage:
30 0e 02 01 00 30 09 0a 01 01 03 04 04 00 00 20

- No.: 1573
- Timestamp: 10:52:29:577_0
- RFN: 2951
- Chip: 7168
- Event: Receive
- PCO: CMAC
- Message: CMAC_SecurityMode_Config_CNF
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 2
- Message Structure:
CMAC_SecurityMode_Config_CNF
. (IntegerType)cellId = 0
- Constraint:
ca_CMAC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 00

- No.: 1574
- Timestamp: 10:52:29:579_0
- RFN: 2951
- Chip: 14336
- Event: Send
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_REQ
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 3
- Message Structure:
CRLC_SecurityMode_Config_REQ
. (IntegerType)cellId = -1
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity = 1
. . (BitStringType)startValue[20] = "00000000000000000010"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = -
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CRLC_SecurityModeCfgReq
- BinaryMessage:
30 0e 02 01 ff 30 09 0a 01 01 03 04 04 00 00 20

- No.: 1575
- Timestamp: 10:52:29:581_0
- RFN: 2951
- Chip: 20736
- Event: Receive
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_CNF
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 4
- Message Structure:
CRLC_SecurityMode_Config_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1589
- Timestamp: 10:52:29:586_0
- RFN: 2952
- Chip: 3328
- Event: Send
- PCO: CMAC
- Message: CMAC_SecurityMode_Config_REQ
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 1
- Message Structure:
CMAC_SecurityMode_Config_REQ
. (IntegerType)cellId = 0
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity = 0
. . (BitStringType)startValue[20] = "00000000000000000010"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = -
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CMAC_SecurityModeCfgReq
- BinaryMessage:
30 0e 02 01 00 30 09 0a 01 00 03 04 04 00 00 20

- No.: 1590
- Timestamp: 10:52:29:588_0
- RFN: 2952
- Chip: 9984
- Event: Receive
- PCO: CMAC
- Message: CMAC_SecurityMode_Config_CNF
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 2
- Message Structure:
CMAC_SecurityMode_Config_CNF
. (IntegerType)cellId = 0
- Constraint:
ca_CMAC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 00

- No.: 1591
- Timestamp: 10:52:29:590_0
- RFN: 2952
- Chip: 17152
- Event: Send
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_REQ
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 3
- Message Structure:
CRLC_SecurityMode_Config_REQ
. (IntegerType)cellId = -1
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity = 0
. . (BitStringType)startValue[20] = "00000000000000000010"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = -
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CRLC_SecurityModeCfgReq
- BinaryMessage:
30 0e 02 01 ff 30 09 0a 01 00 03 04 04 00 00 20

- No.: 1592
- Timestamp: 10:52:29:592_0
- RFN: 2952
- Chip: 23808
- Event: Receive
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_CNF
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 4
- Message Structure:
CRLC_SecurityMode_Config_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1613
- Timestamp: 10:52:29:618_0
- RFN: 2955
- Chip: 8704
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: pr_GenericSetupProcedures:lt_ReceiveResponseToPaging LINE 2
- Message Structure:
RRC_DataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. (START_Value)start[20] = '00000000000000000010'B
. SERVICEREQUEST
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)gMMProtocolDiscriminator[4] = '1000'B
. . (MsgType)msgType[8] = '00001100'B
. . ServiceType_v
. . . (B1)spare1[1] = '0'B
. . . (B3)type[3] = '010'B
. . CiphKeySeqNum
. . . (B1)spare1[1] = '0'B
. . . (KeySeq)keySeq[3] = '000'B
. . MS_Identity_lv
. . . (Length)iel[1] = '05'O
. . . (B4)iDigit1[4] = '1111'B
. . . (B1)oddEvenInd[1] = '0'B
. . . (B3)typeOfId[3] = '100'B
. . . (OctetStringType)otherDigits[4] = '12345678'O
. . PDP_ContextStatus
. . . (IEI8)iei[8] = '00110010'B
. . . (Length)iel[1] = '02'O
. . . (BitStringType)nSAPI[16] = '0000000000000000'B
- Constraint:
car_PS_InitDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 03 04 04 00 00 20 08 0c 20 05 f4 12 34 56 78 32 02 00 00

- No.: 1647
- Timestamp: 10:52:29:632_0
- RFN: 2956
- Chip: 23808
- Event: Send
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_REQ
- Source: ts_SS_DownloadSecurityKey:lt_DownloadKeyCRLC LINE 1
- Message Structure:
CRLC_SecurityMode_Config_REQ
. (IntegerType)cellId = -1
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity = 1
. . (BitStringType)startValue[20] = "00000000000000000010"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = '01010111010101100101000101010000010100110101001001011101010111000101111101011110010110010101100001011011010110100101010101010100'B
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CRLC_SecurityModeCfgReq
- BinaryMessage:
30 21 02 01 ff 30 1c 0a 01 01 03 04 04 00 00 20 03 11 00 57 56 51 50 53 52 5d 5c 5f 5e 59 58 5b 5a 55 54

- No.: 1648
- Timestamp: 10:52:29:634_0
- RFN: 2956
- Chip: 30976
- Event: Receive
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_CNF
- Source: ts_SS_DownloadSecurityKey:lt_DownloadKeyCRLC LINE 2
- Message Structure:
CRLC_SecurityMode_Config_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1655
- Timestamp: 10:52:29:637_0
- RFN: 2957
- Chip: 5120
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 1
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
. (IntegerType)count_I_LSB_UL = -
. (IntegerType)count_I_LSB_DL = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 00 02 01 00 02 01 00

- No.: 1656
- Timestamp: 10:52:29:639_0
- RFN: 2957
- Chip: 12800
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 2
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 00 02 01 00

- No.: 1657
- Timestamp: 10:52:29:641_0
- RFN: 2957
- Chip: 19968
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 3
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. (IntegerType)count_I_LSB_UL = -
. (IntegerType)count_I_LSB_DL = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 01 02 01 00

- No.: 1658
- Timestamp: 10:52:29:643_0
- RFN: 2957
- Chip: 27136
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 4
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 1659
- Timestamp: 10:52:29:644_0
- RFN: 2957
- Chip: 34304
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 5
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. (IntegerType)count_I_LSB_UL = -
. (IntegerType)count_I_LSB_DL = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 02 02 01 00

- No.: 1660
- Timestamp: 10:52:29:646_0
- RFN: 2958
- Chip: 3072
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 6
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 1661
- Timestamp: 10:52:29:648_0
- RFN: 2958
- Chip: 10496
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 7
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
. (IntegerType)count_I_LSB_UL = -
. (IntegerType)count_I_LSB_DL = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 03 02 01 00

- No.: 1662
- Timestamp: 10:52:29:650_0
- RFN: 2958
- Chip: 17664
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 8
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 1663
- Timestamp: 10:52:29:652_0
- RFN: 2958
- Chip: 24832
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 9
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
. (IntegerType)count_I_LSB_UL = -
. (IntegerType)count_I_LSB_DL = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 04 02 01 00

- No.: 1664
- Timestamp: 10:52:29:654_0
- RFN: 2958
- Chip: 32000
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 10
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 1668
- Timestamp: 10:52:29:657_0
- RFN: 2959
- Chip: 4608
- Event: Send
- PCO: CRLC
- Message: CRLC_Integrity_Activate_REQ
- Source: ts_CRLC_DL_Integrity LINE 1
- Message Structure:
CRLC_Integrity_Activate_REQ
. (IntegerType)cellId = -1
. (CN_DomainIdentity)cn_DomainIdentity = 1
. IntegrityActivationInfo
. . IntegrityProtectionModeInfo
. . . IntegrityProtectionModeCommand
. . . . startIntegrityProtection
. . . . . (BitStringType)integrityProtInitNumber[32] = "00000000000000000000000000000001"
. . . (IntegrityProtectionAlgorithm)integrityProtectionAlgorithm = 0
- Constraint:
ca_CRLC_DL_IntegrityActivateReq
- BinaryMessage:
30 15 02 01 ff 0a 01 01 30 0d 30 30 07 03 05 00 00 00 00 01 0a 01 00

- No.: 1669
- Timestamp: 10:52:29:658_0
- RFN: 2959
- Chip: 10752
- Event: Receive
- PCO: CRLC
- Message: CRLC_Integrity_Activate_CNF
- Source: ts_CRLC_DL_Integrity LINE 2
- Message Structure:
CRLC_Integrity_Activate_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_IntegrityActivateCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1676
- Timestamp: 10:52:29:662_0
- RFN: 2959
- Chip: 26112
- Event: Send
- PCO: CRLC
- Message: CRLC_Integrity_Activate_REQ
- Source: ts_RB2_UL_IntegrityActivate LINE 1
- Message Structure:
CRLC_Integrity_Activate_REQ
. (IntegerType)cellId = -1
. (CN_DomainIdentity)cn_DomainIdentity = 1
. IntegrityActivationInfo
. . IntegrityProtActivationInfoList
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity = 2
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
- Constraint:
ca_CRLC_UL_IntegrityActivateReq
- BinaryMessage:
30 10 02 01 ff 0a 01 01 30 08 30 06 02 01 02 02 01 00

- No.: 1677
- Timestamp: 10:52:29:664_0
- RFN: 2959
- Chip: 32000
- Event: Receive
- PCO: CRLC
- Message: CRLC_Integrity_Activate_CNF
- Source: ts_RB2_UL_IntegrityActivate LINE 2
- Message Structure:
CRLC_Integrity_Activate_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_IntegrityActivateCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1683
- Timestamp: 10:52:29:670_0
- RFN: 2960
- Chip: 17920
- Event: Send
- PCO: AM
- Message: RLC_AM_DATA_REQ
- Source: ts_RRC_Security:lt_SendSecurityModeCommand LINE 7
- Message Structure:
RLC_AM_DATA_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. AmConfirmationRequest
. aM_message
. . DL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00000000000000000000000000000000"
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . DL_DCCH_MessageType
. . . . SecurityModeCommand
. . . . . r3
. . . . . . SecurityModeCommand_r3_IEs
. . . . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . . . SecurityCapability
. . . . . . . . (BitStringType)cipheringAlgorithmCap[16] = '0000000000000011'B
. . . . . . . . (BitStringType)integrityProtectionAlgorithmCap[16] = '0000000000000010'B
. . . . . . . CipheringModeInfo
. . . . . . . IntegrityProtectionModeInfo
. . . . . . . . IntegrityProtectionModeCommand
. . . . . . . . . startIntegrityProtection
. . . . . . . . . . (BitStringType)integrityProtInitNumber[32] = "00000000000000000000000000000001"
. . . . . . . . (IntegrityProtectionAlgorithm)integrityProtectionAlgorithm = 0
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity = 1
. . . . . . . InterRAT_UE_SecurityCapList
. . . . . . laterNonCriticalExtensions
- Constraint:
cas_RRC_SecModeCmd
- BinaryMessage:
30 17 02 01 ff 02 01 02 05 00 80 00 00 00 04 04 00 01 80 01 40 00 00 00 30

- No.: 1689
- Timestamp: 10:52:29:799_0
- RFN: 2973
- Chip: 13056
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_IND
- Source: ts_RRC_Security:lt_StartSecurity_UE LINE 8
- Message Structure:
RLC_AM_DATA_IND
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. IntegrityResult
. . (IntegrityStatus)integrityUsed = 0
. aM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "11101101011010000100111100101101"
. . . . (IntegerType)rrc_MessageSequenceNumber = 1
. . . UL_DCCH_MessageType
. . . . SecurityModeComplete
. . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . IntegrityProtActivationInfo
. . . . . . RRC_MessageSequenceNumberList
. . . . . . . (IntegerType)_elem = 0
. . . . . . . (IntegerType)_elem = 0
. . . . . . . (IntegerType)_elem = 0
. . . . . . . (IntegerType)_elem = 0
. . . . . . . (IntegerType)_elem = 0
. . . . . laterNonCriticalExtensions
. . . . . . (BitStringType)securityModeComplete_r3_add_ext = 0
. . . . . . nonCriticalExtensions
- Constraint:
car_RRC_SecModeCmpl
- BinaryMessage:
30 12 02 01 ff 02 01 02 0a 01 00 f6 b4 27 96 8d 21 00 00 00

- No.: 1690
- Timestamp: 10:52:29:800_0
- RFN: 2973
- Chip: 17152
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_Security:lt_StartSecurity_UE LINE 8
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1692
- Timestamp: 10:52:29:804_0
- RFN: 2973
- Chip: 32768
- Event: Send
- PCO: CRLC
- Message: CRLC_Integrity_Activate_REQ
- Source: ts_CRLC_UL_Integrity LINE 1
- Message Structure:
CRLC_Integrity_Activate_REQ
. (IntegerType)cellId = -1
. (CN_DomainIdentity)cn_DomainIdentity = 1
. IntegrityActivationInfo
. . IntegrityProtActivationInfoList
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity = 0
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity = 1
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity = 3
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity = 4
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
- Constraint:
ca_CRLC_UL_IntegrityActivateReq
- BinaryMessage:
30 28 02 01 ff 0a 01 01 30 20 30 06 02 01 00 02 01 00 30 06 02 01 01 02 01 00 30 06 02 01 03 02 01 00 30 06 02 01 04 02 01 00

- No.: 1693
- Timestamp: 10:52:29:806_0
- RFN: 2974
- Chip: 1280
- Event: Receive
- PCO: CRLC
- Message: CRLC_Integrity_Activate_CNF
- Source: ts_CRLC_UL_Integrity LINE 2
- Message Structure:
CRLC_Integrity_Activate_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_IntegrityActivateCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1705
- Timestamp: 10:52:29:839_0
- RFN: 2977
- Chip: 10752
- Event: Send
- PCO: Dc
- Message: RRC_DataReq
- Source: ts_TC_ActivateRB_TestMode LINE 7
- Message Structure:
RRC_DataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[-1] = -
. (SapId)sapId[1] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. ACTIVATERBTESTMODE
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)tCProtocolDiscriminator[4] = '1111'B
. . (MsgType)msgType[8] = '01000100'B
- Constraint:
ca_PS_DataReq
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 0f 44

- No.: 1706
- Timestamp: 10:52:29:840_0
- RFN: 2977
- Chip: 14336
- Event: Start Timer
- Source: ts_TC_ActivateRB_TestMode LINE 7
- Message Structure:
no details available
- Constraint:
t_Dly (5000 Ms)
- BinaryMessage:

- No.: 1710
- Timestamp: 10:52:29:966_0
- RFN: 2990
- Chip: 3840
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_TC_ActivateRB_TestMode LINE 8
- Message Structure:
RRC_DataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. (START_Value)start[0] = -
. ACTIVATERBTESTMODECOMPLETE
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)tCProtocolDiscriminator[4] = '1111'B
. . (MsgType)msgType[8] = '01000101'B
- Constraint:
car_PS_UplinkDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 0f 45

- No.: 1711
- Timestamp: 10:52:29:968_0
- RFN: 2990
- Chip: 8192
- Event: Cancel Timer
- Source: ts_TC_ActivateRB_TestMode LINE 8
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 1712
- Timestamp: 10:52:29:968_1
- RFN: 2990
- Chip: 8960
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_TC_ActivateRB_TestMode LINE 8
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1731
- Timestamp: 10:52:30:009_0
- RFN: 2994
- Chip: 9984
- Event: Send
- PCO: CPHY
- Message: CPHY_Frame_Number_REQ
- Source: ts_RRC_SetUpRAB_AM_7_RLC LINE 2
- Message Structure:
CPHY_Frame_Number_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
cas_GetFrameNum
- BinaryMessage:
30 06 02 01 00 02 01 1a

- No.: 1735
- Timestamp: 10:52:30:051_0
- RFN: 2998
- Chip: 19968
- Event: Receive
- PCO: CPHY
- Message: CPHY_Frame_Number_CNF
- Source: ts_RRC_SetUpRAB_AM_7_RLC LINE 3
- Message Structure:
CPHY_Frame_Number_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
. (IntegerType)frameNumber = 178
- Constraint:
car_GetFrameNum
- BinaryMessage:
30 0a 02 01 00 02 01 1a 02 02 00 b2

- No.: 1739
- Timestamp: 10:52:30:149_0
- RFN: 3008
- Chip: 11008
- Event: Send
- PCO: AM
- Message: RLC_AM_DATA_REQ
- Source: ts_RRC_SetUpRAB_AM_7_RLC:lt_SendRAB_SetupCS_OrPS LINE 4
- Message Structure:
RLC_AM_DATA_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. AmConfirmationRequest
. . (IntegerType)confirmationRequested = 0
. aM_message
. . DL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00000000000000000000000000000000"
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . DL_DCCH_MessageType
. . . . RadioBearerSetup
. . . . . r3
. . . . . . RadioBearerSetup_r3_IEs
. . . . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . . . IntegrityProtectionModeInfo
. . . . . . . CipheringModeInfo
. . . . . . . (IntegerType)activationTime = 168
. . . . . . . U_RNTI
. . . . . . . (BitStringType)new_C_RNTI[16] = -
. . . . . . . (RRC_StateIndicator)rrc_StateIndicator = 0
. . . . . . . (IntegerType)utran_DRX_CycleLengthCoeff = -
. . . . . . . (BitStringType)ura_Identity[0] = -
. . . . . . . CN_InformationInfo
. . . . . . . SRB_InformationSetupList
. . . . . . . RAB_InformationSetupList
. . . . . . . . RAB_InformationSetup
. . . . . . . . . RAB_Info
. . . . . . . . . . RAB_Identity
. . . . . . . . . . . (BitStringType)gsm_MAP_RAB_Identity[8] = '00000101'B
. . . . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = 1
. . . . . . . . . . (BitStringType)nas_Synchronisation_Indicator[0] = -
. . . . . . . . . . (Re_EstablishmentTimer)re_EstablishmentTimer = 0
. . . . . . . . . RB_InformationSetupList
. . . . . . . . . . RB_InformationSetup
. . . . . . . . . . . (IntegerType)rb_Identity = 20
. . . . . . . . . . . PDCP_Info
. . . . . . . . . . . RLC_InfoChoice
. . . . . . . . . . . . RLC_Info
. . . . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . . . MaxDAT_Retransmissions
. . . . . . . . . . . . . . . . . (MaxDAT)maxDAT = 3
. . . . . . . . . . . . . . . . . (TimerMRW)timerMRW = 13
. . . . . . . . . . . . . . . . . (MaxMRW)maxMRW = 1
. . . . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize = 5
. . . . . . . . . . . . . . . (TimerRST)timerRST = 9
. . . . . . . . . . . . . . . (MaxRST)max_RST = 1
. . . . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit = -
. . . . . . . . . . . . . . . . (TimerPoll)timerPoll = -
. . . . . . . . . . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . . . . . . . . . (Poll_SDU)poll_SDU = -
. . . . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = FALSE
. . . . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = FALSE
. . . . . . . . . . . . . . . . (PollWindow)pollWindow = -
. . . . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic = 4
. . . . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize = 5
. . . . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit = -
. . . . . . . . . . . . . . . . (TimerEPC)timerEPC = -
. . . . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . . . . . . . . RB_MappingInfo
. . . . . . . . . . . . RB_MappingOption
. . . . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . . . (IntegerType)dch = 1
. . . . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 7
. . . . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 7
. . . . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . . . (IntegerType)dch = 6
. . . . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 7
. . . . . . . RB_InformationAffectedList
. . . . . . . DL_CounterSynchronisationInfo
. . . . . . . UL_CommonTransChInfo
. . . . . . . . TFC_Subset
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . TFCS
. . . . . . . . . . . ExplicitTFCS_Configuration
. . . . . . . . . . . . TFCS_ReconfAdd
. . . . . . . . . . . . . ctfcSize
. . . . . . . . . . . . . . ctfc4Bit
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . . . . . . . (IntegerType)ctfc4 = 0
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . . . . . . . (IntegerType)ctfc4 = 1
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . . . . . . . (IntegerType)ctfc4 = 2
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . . . . . . . (IntegerType)ctfc4 = 3
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 11
. . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . UL_DeletedTransChInfoList
. . . . . . . UL_AddReconfTransChInfoList
. . . . . . . . UL_AddReconfTransChInformation
. . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType = 0
. . . . . . . . . (IntegerType)transportChannelIdentity = 1
. . . . . . . . . TransportFormatSet
. . . . . . . . . . DedicatedTransChTFS
. . . . . . . . . . . tti
. . . . . . . . . . . . DedicatedDynamicTF_InfoList
. . . . . . . . . . . . . DedicatedDynamicTF_Info
. . . . . . . . . . . . . . rlc_Size
. . . . . . . . . . . . . . . OctetModeRLC_SizeInfoType1
. . . . . . . . . . . . . . . . (IntegerType)sizeType1 = 16
. . . . . . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . LogicalChannelList
. . . . . . . . . . . SemistaticTF_Information
. . . . . . . . . . . . ChannelCodingType
. . . . . . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . . . . . (IntegerType)rateMatchingAttribute = 155
. . . . . . . . . . . . (CRC_Size)crc_Size = 3
. . . . . . . . UL_AddReconfTransChInformation
. . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType = 0
. . . . . . . . . (IntegerType)transportChannelIdentity = 5
. . . . . . . . . TransportFormatSet
. . . . . . . . . . DedicatedTransChTFS
. . . . . . . . . . . tti
. . . . . . . . . . . . DedicatedDynamicTF_InfoList
. . . . . . . . . . . . . DedicatedDynamicTF_Info
. . . . . . . . . . . . . . rlc_Size
. . . . . . . . . . . . . . . BitModeRLC_SizeInfo
. . . . . . . . . . . . . . . . sizeType2
. . . . . . . . . . . . . . . . . (IntegerType)part1 = 2
. . . . . . . . . . . . . . . . . (IntegerType)part2 = -
. . . . . . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . LogicalChannelList
. . . . . . . . . . . SemistaticTF_Information
. . . . . . . . . . . . ChannelCodingType
. . . . . . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . . . . . (IntegerType)rateMatchingAttribute = 170
. . . . . . . . . . . . (CRC_Size)crc_Size = 3
. . . . . . . modeSpecificTransChInfo
. . . . . . . . fdd
. . . . . . . . . (IntegerType)cpch_SetID = -
. . . . . . . . . DRAC_StaticInformationList
. . . . . . . DL_CommonTransChInfo
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . dl_Parameters
. . . . . . . DL_DeletedTransChInfoList
. . . . . . . DL_AddReconfTransChInfoList
. . . . . . . . DL_AddReconfTransChInformation
. . . . . . . . . (DL_TrCH_Type)dl_TransportChannelType = 0
. . . . . . . . . (IntegerType)dl_transportChannelIdentity = 6
. . . . . . . . . tfs_SignallingMode
. . . . . . . . . . UL_TransportChannelIdentity
. . . . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType = 0
. . . . . . . . . . . (IntegerType)ul_TransportChannelIdentity = 1
. . . . . . . . . QualityTarget
. . . . . . . . . . (IntegerType)bler_QualityValue = -20
. . . . . . . . . TM_SignallingInfo
. . . . . . . . DL_AddReconfTransChInformation
. . . . . . . . . (DL_TrCH_Type)dl_TransportChannelType = 0
. . . . . . . . . (IntegerType)dl_transportChannelIdentity = 10
. . . . . . . . . tfs_SignallingMode
. . . . . . . . . . UL_TransportChannelIdentity
. . . . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType = 0
. . . . . . . . . . . (IntegerType)ul_TransportChannelIdentity = 5
. . . . . . . . . QualityTarget
. . . . . . . . . . (IntegerType)bler_QualityValue = -20
. . . . . . . . . TM_SignallingInfo
. . . . . . . FrequencyInfo
. . . . . . . (IntegerType)maxAllowedUL_TX_Power = 33
. . . . . . . UL_ChannelRequirement
. . . . . . . . UL_DPCH_Info
. . . . . . . . . UL_DPCH_PowerControlInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (IntegerType)dpcch_PowerOffset = -40
. . . . . . . . . . . (IntegerType)pc_Preamble = 1
. . . . . . . . . . . (IntegerType)sRB_delay = 7
. . . . . . . . . . . PowerControlAlgorithm
. . . . . . . . . . . . (IntegerType)algorithm1 = 1
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (ScramblingCodeType)scramblingCodeType = 1
. . . . . . . . . . . (IntegerType)scramblingCode = 0
. . . . . . . . . . . (IntegerType)numberOfDPDCH = -
. . . . . . . . . . . (SpreadingFactor)spreadingFactor = 4
. . . . . . . . . . . (BooleanType)tfci_Existence = TRUE
. . . . . . . . . . . (IntegerType)numberOfFBI_Bits = -
. . . . . . . . . . . (PuncturingLimit)puncturingLimit = 15
. . . . . . . modeSpecificPhysChInfo
. . . . . . . . fdd
. . . . . . . . . DL_PDSCH_Information
. . . . . . . DL_CommonInformation
. . . . . . . . DL_DPCH_InfoCommon
. . . . . . . . . cfnHandling
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . DL_DPCH_PowerControlInfo
. . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . (DPC_Mode)dpc_Mode = 0
. . . . . . . . . . . (IntegerType)powerOffsetPilot_pdpdch = 0
. . . . . . . . . . . Dl_rate_matching_restriction
. . . . . . . . . . . SF512_AndPilot
. . . . . . . . . . . . (PilotBits128)sfd128 = 0
. . . . . . . . . . . (PositionFixedOrFlexible)positionFixedOrFlexible = 1
. . . . . . . . . . . (BooleanType)tfci_Existence = TRUE
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . (IntegerType)defaultDPCH_OffsetValue = -
. . . . . . . . . . DPCH_CompressedModeInfo
. . . . . . . . . . (TX_DiversityMode)tx_DiversityMode = 0
. . . . . . . . . . SSDT_Information
. . . . . . . DL_InformationPerRL_List
. . . . . . . . DL_InformationPerRL
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . PrimaryCPICH_Info
. . . . . . . . . . . . (IntegerType)primaryScramblingCode = 100
. . . . . . . . . . . PDSCH_SHO_DCH_Info
. . . . . . . . . . . PDSCH_CodeMapping
. . . . . . . . . DL_DPCH_InfoPerRL
. . . . . . . . . . fdd
. . . . . . . . . . . (PCPICH_UsageForChannelEst)pCPICH_UsageForChannelEst = 0
. . . . . . . . . . . (IntegerType)dpch_FrameOffset = 0
. . . . . . . . . . . SecondaryCPICH_Info
. . . . . . . . . . . DL_ChannelisationCodeList
. . . . . . . . . . . . DL_ChannelisationCode
. . . . . . . . . . . . . (IntegerType)secondaryScramblingCode = 1
. . . . . . . . . . . . . SF512_AndCodeNumber
. . . . . . . . . . . . . . (IntegerType)sf128 = 0
. . . . . . . . . . . . . (ScramblingCodeChange)scramblingCodeChange = -
. . . . . . . . . . . (IntegerType)tpc_CombinationIndex = 0
. . . . . . . . . . . (SSDT_CellIdentity)ssdt_CellIdentity = -
. . . . . . . . . . . (ClosedLoopTimingAdjMode)closedLoopTimingAdjMode = -
. . . . . . . . . SCCPCH_InfoForFACH
. . . . . . v3a0NonCriticalExtensions
. . . . . . . RadioBearerSetup_v3a0ext
. . . . . . . . (BitStringType)new_DSCH_RNTI[16] = -
. . . . . . . laterNonCriticalExtensions
- Constraint:
cas_RB_SetUpAM_WithCnf
- BinaryMessage:
30 4f 02 01 ff 02 01 02 02 01 00 80 00 00 00 03 92 04 ba f2 a0 00 16 09 b3 1e 95 92 09 0a 88 d0 0c e4 2b 10 20 1c 12 29 24 99 5f 81 00 41 20 11 1c d3 10 80 44 11 1d 4b 06 18 58 15 c4 c4 ae 9a 54 7a 20 00 00 13 e4 80 56 20 40 c8 00 01 05 00 00

- No.: 1744
- Timestamp: 10:52:30:329_0
- RFN: 3026
- Chip: 11008
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_CNF
- Source: ts_RRC_SetUpRAB_AM_7_RLC LINE 6
- Message Structure:
RLC_AM_DATA_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. (IntegerType)mui = 0
- Constraint:
car_AM_DataMuiCnf
- BinaryMessage:
30 09 02 01 ff 02 01 02 02 01 00

- No.: 1751
- Timestamp: 10:52:30:464_0
- RFN: 3039
- Chip: 32000
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Modify_REQ
- Source: ts_SS_2DCH_Modify LINE 3
- Message Structure:
CPHY_RL_Modify_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
. (RatType)ratType = 0
. CphyRlModifyReq
. . SS_ActivationTime
. . . (IntegerType)activationCFN = 168
. . physicalChannelInfo
. . . DPCHInfo
. . . . UL_DPCH_Info
. . . . DL_DPCHInfo
. . . . . DL_CommonInformation
. . . . . . DL_DPCH_InfoCommon
. . . . . . . cfnHandling
. . . . . . . modeSpecificInfo
. . . . . . . . fdd
. . . . . . . . . DL_DPCH_PowerControlInfo
. . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . fdd
. . . . . . . . . . . . (DPC_Mode)dpc_Mode = 0
. . . . . . . . . (IntegerType)powerOffsetPilot_pdpdch = 0
. . . . . . . . . Dl_rate_matching_restriction
. . . . . . . . . SF512_AndPilot
. . . . . . . . . . (PilotBits128)sfd128 = 0
. . . . . . . . . (PositionFixedOrFlexible)positionFixedOrFlexible = 1
. . . . . . . . . (BooleanType)tfci_Existence = TRUE
. . . . . . modeSpecificInfo
. . . . . . . fdd
. . . . . . . . (IntegerType)defaultDPCH_OffsetValue = -
. . . . . . . . DPCH_CompressedModeInfo
. . . . . . . . (TX_DiversityMode)tx_DiversityMode = 0
. . . . . . . . SSDT_Information
. . . . . DL_DPCH_InfoPerRL
. . . . . . fdd
. . . . . . . (PCPICH_UsageForChannelEst)pCPICH_UsageForChannelEst = 0
. . . . . . . (IntegerType)dpch_FrameOffset = 0
. . . . . . . SecondaryCPICH_Info
. . . . . . . DL_ChannelisationCodeList
. . . . . . . . DL_ChannelisationCode
. . . . . . . . . (IntegerType)secondaryScramblingCode = 1
. . . . . . . . . SF512_AndCodeNumber
. . . . . . . . . . (IntegerType)sf128 = 0
. . . . . . . . . (ScramblingCodeChange)scramblingCodeChange = -
. . . . . . . (IntegerType)tpc_CombinationIndex = 0
. . . . . . . (SSDT_CellIdentity)ssdt_CellIdentity = -
. . . . . . . (ClosedLoopTimingAdjMode)closedLoopTimingAdjMode = -
. . . . . (IntegerType)powerOffsetOfTFCI_PO1 = 0
. . . . . (IntegerType)powerOffsetOfTPC_PO2 = 0
. . . . . (IntegerType)powerOffsetOfPILOT_PO3 = 0
. . . . . (IntegerType)dl_TxPower = -5
. . . . . (IntegerType)dl_TxPowerMax = 15
. . . . . (IntegerType)dl_TxPowerMin = -35
- Constraint:
ca_DL_DPCH_ModifyInfo
- BinaryMessage:
30 5e 02 01 00 02 01 1a 0a 01 00 30 53 02 02 00 a8 30 4d 30 4b 30 21 30 19 05 00 30 30 14 30 06 30 30 03 0a 01 00 02 01 00 0a 01 00 0a 01 01 01 01 ff 30 30 03 0a 01 00 30 30 13 0a 01 00 02 01 00 30 08 30 06 02 01 01 02 01 00 02 01 00 02 01 00 02 01 00 02 01 00 02 01 fb 02 01 0f 02 01 dd

- No.: 1755
- Timestamp: 10:52:30:519_0
- RFN: 3045
- Chip: 12544
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Modify_CNF
- Source: ts_SS_2DCH_Modify LINE 4
- Message Structure:
CPHY_RL_Modify_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
ca_RL_ModifyCnf
- BinaryMessage:
30 06 02 01 00 02 01 1a

- No.: 1756
- Timestamp: 10:52:30:549_0
- RFN: 3048
- Chip: 11776
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Config_REQ
- Source: ts_SS_2DCH_Modify LINE 5
- Message Structure:
CPHY_TrCH_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
. (RatType)ratType = 0
. CphyTrchConfigReq
. . SS_ActivationTime
. . . (IntegerType)activationCFN = 168
. . ulconnectedTrCHList
. . TFCS
. . dlconnectedTrCHList
. . . CphyTrchConfigReq_setseq_1
. . . . (IntegerType)trchid = 6
. . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 144
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional = 1
. . . . . . (IntegerType)rateMatchingAttribute = 155
. . . . . . (CRC_Size)crc_Size = 3
. . . CphyTrchConfigReq_setseq_1
. . . . (IntegerType)trchid = 10
. . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 148
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional = 1
. . . . . . (IntegerType)rateMatchingAttribute = 170
. . . . . . (CRC_Size)crc_Size = 3
. . TFCS
. . . ExplicitTFCS_Configuration
. . . . TFCS_ReconfAdd
. . . . . ctfcSize
. . . . . . ctfc4Bit
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 0
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 1
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 2
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 3
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . fdd
. . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 9
. . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
- Constraint:
ca_TrChCfgInfo
- BinaryMessage:
30 81 96 02 01 00 02 01 1a 0a 01 00 30 81 8a 02 02 00 a8 30 4c 30 24 02 01 06 0a 01 00 30 1c 30 0e 30 0c 02 02 00 90 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 9b 0a 01 03 30 24 02 01 0a 0a 01 00 30 1c 30 0e 30 0c 02 02 00 94 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 aa 0a 01 03 30 36 30 30 33 30 08 02 01 00 30 03 02 01 00 30 08 02 01 01 30 03 02 01 00 30 08 02 01 02 30 03 02 01 00 30 13 02 01 03 30 0e 30 0c 30 30 03 02 01 09 02 01 0f 02 01 00

- No.: 1760
- Timestamp: 10:52:30:606_0
- RFN: 3054
- Chip: 3328
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Config_CNF
- Source: ts_SS_2DCH_Modify LINE 6
- Message Structure:
CPHY_TrCH_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
ca_TrChCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 1a

- No.: 1761
- Timestamp: 10:52:30:668_0
- RFN: 3060
- Chip: 7424
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_SS_2DCH_Modify LINE 7
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
. (RatType)ratType = 0
. configMessage
. . CmacConfigReq
. . . SS_ActivationTime
. . . . (IntegerType)activationCFN = 168
. . . UE_Info
. . . . U_RNTI
. . . . (BitStringType)c_RNTI[16] = -
. . . TrCHInfo
. . . . ulconnectedTrCHList
. . . . TFCS
. . . . dlconnectedTrCHList
. . . . . TrCHInfo_setseq_1
. . . . . . (IntegerType)trchid = 6
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 144
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . (IntegerType)rateMatchingAttribute = 155
. . . . . . . . (CRC_Size)crc_Size = 3
. . . . . TrCHInfo_setseq_1
. . . . . . (IntegerType)trchid = 10
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 148
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . (IntegerType)rateMatchingAttribute = 170
. . . . . . . . (CRC_Size)crc_Size = 3
. . . . TFCS
. . . . . ExplicitTFCS_Configuration
. . . . . . TFCS_ReconfAdd
. . . . . . . ctfcSize
. . . . . . . . ctfc4Bit
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 0
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 1
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 2
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 3
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 9
. . . . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . TrCH_LogCHMappingList1
. . . . ulconnectedTrCHList
. . . . dlconnectedTrCHList
. . . . . TrCH_LogCHMappingList1_setseq_1
. . . . . . (IntegerType)trchid = 6
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 7
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 5
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 7
. . . . . . . . (IntegerType)rB_Identity = -12
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . TrCH_LogCHMappingList1_setseq_1
. . . . . . (IntegerType)trchid = 10
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 1
. . . . . . . . (IntegerType)rB_Identity = 1
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 2
. . . . . . . . (IntegerType)rB_Identity = 2
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 3
. . . . . . . . (IntegerType)rB_Identity = 3
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 4
. . . . . . . . (IntegerType)rB_Identity = 4
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_CMAC_ReconfigInfo
- BinaryMessage:
30 82 01 22 02 01 ff 02 01 1a 0a 01 00 30 82 01 15 02 02 00 a8 30 00 30 81 80 30 46 30 21 02 01 06 30 1c 30 0e 30 0c 02 02 00 90 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 9b 0a 01 03 30 21 02 01 0a 30 1c 30 0e 30 0c 02 02 00 94 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 aa 0a 01 03 30 36 30 30 33 30 08 02 01 00 30 03 02 01 00 30 08 02 01 01 30 03 02 01 00 30 08 02 01 02 30 03 02 01 00 30 13 02 01 03 30 0e 30 0c 30 30 03 02 01 09 02 01 0f 02 01 00 30 81 89 30 81 86 30 1d 02 01 06 30 18 30 16 30 11 0a 01 00 0a 01 00 02 01 07 0a 01 05 05 00 02 01 07 02 01 f4 30 65 02 01 0a 30 60 30 16 30 11 0a 01 00 0a 01 00 02 01 01 0a 01 04 05 00 02 01 01 02 01 01 30 16 30 11 0a 01 00 0a 01 00 02 01 02 0a 01 04 05 00 02 01 02 02 01 02 30 16 30 11 0a 01 00 0a 01 00 02 01 03 0a 01 04 05 00 02 01 03 02 01 03 30 16 30 11 0a 01 00 0a 01 00 02 01 04 0a 01 04 05 00 02 01 04 02 01 04

- No.: 1762
- Timestamp: 10:52:30:704_0
- RFN: 3063
- Chip: 29952
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_SS_2DCH_Modify LINE 8
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 1a

- No.: 1763
- Timestamp: 10:52:30:731_0
- RFN: 3066
- Chip: 20480
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Modify_REQ
- Source: ts_SS_2DCH_Modify LINE 9
- Message Structure:
CPHY_RL_Modify_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
. (RatType)ratType = 0
. CphyRlModifyReq
. . SS_ActivationTime
. . . (IntegerType)activationCFN = 168
. . physicalChannelInfo
. . . DPCHInfo
. . . . UL_DPCH_Info
. . . . . UL_DPCH_PowerControlInfo
. . . . . . fdd
. . . . . . . (IntegerType)dpcch_PowerOffset = -40
. . . . . . . (IntegerType)pc_Preamble = 1
. . . . . . . (IntegerType)sRB_delay = 7
. . . . . . . PowerControlAlgorithm
. . . . . . . . (IntegerType)algorithm1 = 1
. . . . . modeSpecificInfo
. . . . . . fdd
. . . . . . . (ScramblingCodeType)scramblingCodeType = 1
. . . . . . . (IntegerType)scramblingCode = 0
. . . . . . . (IntegerType)numberOfDPDCH = -
. . . . . . . (SpreadingFactor)spreadingFactor = 4
. . . . . . . (BooleanType)tfci_Existence = TRUE
. . . . . . . (IntegerType)numberOfFBI_Bits = -
. . . . . . . (PuncturingLimit)puncturingLimit = 15
. . . . DL_DPCHInfo
- Constraint:
ca_UL_DPCH_ModifyInfo
- BinaryMessage:
30 34 02 01 00 02 01 14 0a 01 00 30 29 02 02 00 a8 30 23 30 21 30 30 0c 02 01 d8 02 01 01 02 01 07 02 01 01 30 30 0f 0a 01 01 02 01 00 0a 01 04 01 01 ff 0a 01 0f

- No.: 1767
- Timestamp: 10:52:30:783_0
- RFN: 3071
- Chip: 26880
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Modify_CNF
- Source: ts_SS_2DCH_Modify LINE 10
- Message Structure:
CPHY_RL_Modify_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_RL_ModifyCnf
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 1768
- Timestamp: 10:52:30:813_0
- RFN: 3074
- Chip: 28416
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Config_REQ
- Source: ts_SS_2DCH_Modify LINE 11
- Message Structure:
CPHY_TrCH_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
. (RatType)ratType = 0
. CphyTrchConfigReq
. . SS_ActivationTime
. . . (IntegerType)activationCFN = 168
. . ulconnectedTrCHList
. . . CphyTrchConfigReq_setseq_0
. . . . (IntegerType)trchid = 1
. . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 144
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional = 1
. . . . . . (IntegerType)rateMatchingAttribute = 155
. . . . . . (CRC_Size)crc_Size = 3
. . . CphyTrchConfigReq_setseq_0
. . . . (IntegerType)trchid = 5
. . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 148
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional = 1
. . . . . . (IntegerType)rateMatchingAttribute = 170
. . . . . . (CRC_Size)crc_Size = 3
. . TFCS
. . . ExplicitTFCS_Configuration
. . . . TFCS_ReconfAdd
. . . . . ctfcSize
. . . . . . ctfc4Bit
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 0
. . . . . . . . PowerOffsetInformation
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 1
. . . . . . . . PowerOffsetInformation
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 2
. . . . . . . . PowerOffsetInformation
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 3
. . . . . . . . PowerOffsetInformation
. . dlconnectedTrCHList
. . TFCS
- Constraint:
ca_TrChCfgInfo
- BinaryMessage:
30 76 02 01 00 02 01 14 0a 01 00 30 6b 02 02 00 a8 30 4c 30 24 02 01 01 0a 01 00 30 1c 30 0e 30 0c 02 02 00 90 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 9b 0a 01 03 30 24 02 01 05 0a 01 00 30 1c 30 0e 30 0c 02 02 00 94 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 aa 0a 01 03 30 17 30 30 14 30 03 02 01 00 30 03 02 01 01 30 03 02 01 02 30 03 02 01 03

- No.: 1772
- Timestamp: 10:52:30:864_0
- RFN: 3079
- Chip: 33536
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Config_CNF
- Source: ts_SS_2DCH_Modify LINE 12
- Message Structure:
CPHY_TrCH_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_TrChCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 1773
- Timestamp: 10:52:30:928_0
- RFN: 3086
- Chip: 11520
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_SS_2DCH_Modify LINE 13
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
. (RatType)ratType = 0
. configMessage
. . CmacConfigReq
. . . SS_ActivationTime
. . . . (IntegerType)activationCFN = 168
. . . UE_Info
. . . . U_RNTI
. . . . (BitStringType)c_RNTI[16] = -
. . . TrCHInfo
. . . . ulconnectedTrCHList
. . . . . TrCHInfo_setseq_0
. . . . . . (IntegerType)trchid = 1
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 144
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . (IntegerType)rateMatchingAttribute = 155
. . . . . . . . (CRC_Size)crc_Size = 3
. . . . . TrCHInfo_setseq_0
. . . . . . (IntegerType)trchid = 5
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 148
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . (IntegerType)rateMatchingAttribute = 170
. . . . . . . . (CRC_Size)crc_Size = 3
. . . . TFCS
. . . . . ExplicitTFCS_Configuration
. . . . . . TFCS_ReconfAdd
. . . . . . . ctfcSize
. . . . . . . . ctfc4Bit
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 0
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 1
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 2
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 3
. . . . . . . . . . PowerOffsetInformation
. . . . dlconnectedTrCHList
. . . . TFCS
. . . TrCH_LogCHMappingList1
. . . . ulconnectedTrCHList
. . . . . TrCH_LogCHMappingList1_setseq_0
. . . . . . (IntegerType)trchid = 1
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 7
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 5
. . . . . . . . (IntegerType)rB_Identity = -12
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . TrCH_LogCHMappingList1_setseq_0
. . . . . . (IntegerType)trchid = 5
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . (IntegerType)rB_Identity = 1
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . (IntegerType)rB_Identity = 2
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . (IntegerType)rB_Identity = 3
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . (IntegerType)rB_Identity = 4
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . dlconnectedTrCHList
- Constraint:
ca_CMAC_ReconfigInfo
- BinaryMessage:
30 81 e6 02 01 ff 02 01 14 0a 01 00 30 81 da 02 02 00 a8 30 00 30 61 30 46 30 21 02 01 01 30 1c 30 0e 30 0c 02 02 00 90 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 9b 0a 01 03 30 21 02 01 05 30 1c 30 0e 30 0c 02 02 00 94 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 aa 0a 01 03 30 17 30 30 14 30 03 02 01 00 30 03 02 01 01 30 03 02 01 02 30 03 02 01 03 30 6f 30 6d 30 18 02 01 01 30 13 30 11 30 0c 0a 01 00 0a 01 00 02 01 07 0a 01 05 02 01 f4 30 51 02 01 05 30 4c 30 11 30 0c 0a 01 00 0a 01 00 02 01 01 0a 01 04 02 01 01 30 11 30 0c 0a 01 00 0a 01 00 02 01 02 0a 01 04 02 01 02 30 11 30 0c 0a 01 00 0a 01 00 02 01 03 0a 01 04 02 01 03 30 11 30 0c 0a 01 00 0a 01 00 02 01 04 0a 01 04 02 01 04

- No.: 1777
- Timestamp: 10:52:30:984_0
- RFN: 3091
- Chip: 28928
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_SS_2DCH_Modify LINE 14
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 14

- No.: 1780
- Timestamp: 10:52:30:995_0
- RFN: 3092
- Chip: 33792
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB_TM_Cfg_RLC LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = -12
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_TM_RLC_Mode
. . . . . . (BooleanType)segmentationIndication = TRUE
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 144
. . . . . UL_RLC_Mode
. . . . . . UL_TM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . (BooleanType)segmentationIndication = TRUE
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = 7
. . . . (IntegerType)dLlogicalChannelIdentity = 7
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_TM_Info
- BinaryMessage:
30 25 02 01 ff 02 01 f4 0a 01 00 30 1a 30 10 30 03 01 01 ff 30 09 02 02 00 90 30 03 01 01 ff 30 06 02 01 07 02 01 07

- No.: 1784
- Timestamp: 10:52:31:008_0
- RFN: 3094
- Chip: 7168
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB_TM_Cfg_RLC LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = -12
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 f4

- No.: 1792
- Timestamp: 10:52:31:038_0
- RFN: 3097
- Chip: 7424
- Event: Start Timer
- Source: ts_RRC_ReceiveRB_SetupCmpl LINE 2
- Message Structure:
no details available
- Constraint:
t_WaitMS (13500 Ms)
- BinaryMessage:

- No.: 1801
- Timestamp: 10:52:32:580_0
- RFN: 3251
- Chip: 15104
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_IND
- Source: ts_RRC_ReceiveRB_SetupCmpl:lt_CipheringNotStartedAM_RAB LINE 4
- Message Structure:
RLC_AM_DATA_IND
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. IntegrityResult
. . (IntegrityStatus)integrityUsed = 0
. aM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "01100111110100110110111001101110"
. . . . (IntegerType)rrc_MessageSequenceNumber = 2
. . . UL_DCCH_MessageType
. . . . RadioBearerSetupComplete
. . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . IntegrityProtActivationInfo
. . . . . (IntegerType)ul_TimingAdvance = 0
. . . . . (BitStringType)start_Value[20] = "00000000000000000100"
. . . . . (IntegerType)count_C_ActivationTime = 0
. . . . . UL_CounterSynchronisationInfo
. . . . . laterNonCriticalExtensions
. . . . . . (BitStringType)radioBearerSetupComplete_r3_add_ext = 0
. . . . . . nonCriticalExtensions
- Constraint:
car_RB_SetUpCmpl
- BinaryMessage:
30 12 02 01 ff 02 01 02 0a 01 00 b3 e9 b7 37 13 c8 00 00 08

- No.: 1802
- Timestamp: 10:52:32:581_0
- RFN: 3251
- Chip: 20736
- Event: Cancel Timer
- Source: ts_RRC_ReceiveRB_SetupCmpl:lt_CipheringNotStartedAM_RAB LINE 4
- Message Structure:
no details available
- Constraint:
t_WaitMS
- BinaryMessage:

- No.: 1803
- Timestamp: 10:52:32:582_0
- RFN: 3251
- Chip: 21760
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ReceiveRB_SetupCmpl:lt_CipheringNotStartedAM_RAB LINE 4
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1832
- Timestamp: 10:52:32:638_0
- RFN: 3257
- Chip: 7936
- Event: Send
- PCO: Dc
- Message: RRC_DataReq
- Source: ts_TC_CloseUE_TestLoop LINE 6
- Message Structure:
RRC_DataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[-1] = -
. (SapId)sapId[1] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. CLOSEUETESTLOOP
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)tCProtocolDiscriminator[4] = '1111'B
. . (MsgType)msgType[8] = '01000000'B
. . (UE_TestLoopMode)uE_TestLoopMode[1] = '00'O
. . UE_TestLoopMode1LB_Setup
. . . (Length)iel[1] = '03'O
. . . LB_SetupRB_IE
. . . . (BitStringType)rLC_SDU_Size[16] = '0000001001111000'B
. . . . (BitStringType)spare_2[3] = '000'B
. . . . (BitStringType)rB_Identity[5] = '10100'B
. . . LB_SetupRB_IE
. . . LB_SetupRB_IE
. . . LB_SetupRB_IE
- Constraint:
ca_PS_DataReq
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 0f 40 00 03 02 78 14

- No.: 1833
- Timestamp: 10:52:32:639_0
- RFN: 3257
- Chip: 13312
- Event: Start Timer
- Source: ts_TC_CloseUE_TestLoop LINE 6
- Message Structure:
no details available
- Constraint:
t_Dly (5000 Ms)
- BinaryMessage:

- No.: 1837
- Timestamp: 10:52:32:930_0
- RFN: 3286
- Chip: 13568
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_TC_CloseUE_TestLoop LINE 7
- Message Structure:
RRC_DataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. (START_Value)start[0] = -
. CLOSEUETESTLOOPCOMPLETE
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)tCProtocolDiscriminator[4] = '1111'B
. . (MsgType)msgType[8] = '01000001'B
- Constraint:
car_PS_UplinkDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 0f 41

- No.: 1838
- Timestamp: 10:52:32:930_1
- RFN: 3286
- Chip: 16896
- Event: Cancel Timer
- Source: ts_TC_CloseUE_TestLoop LINE 7
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 1839
- Timestamp: 10:52:32:931_0
- RFN: 3286
- Chip: 17664
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_TC_CloseUE_TestLoop LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1847
- Timestamp: 10:52:32:942_1
- RFN: 3287
- Chip: 23296
- Event: Start Timer
- Source: tc_7_2_3_19:lt_MonitorUplink LINE 1
- Message Structure:
no details available
- Constraint:
t_WaitMS (1000 Ms)
- BinaryMessage:

- No.: 1851
- Timestamp: 10:52:33:936_0
- RFN: 3387
- Chip: 2304
- Event: Timeout
- Source: tc_7_2_3_19:lt_MonitorUplink LINE 3
- Message Structure:
no details available
- Constraint:
t_WaitMS
- BinaryMessage:

- No.: 1858
- Timestamp: 10:52:33:946_0
- RFN: 3388
- Chip: 512
- Event: Start Timer
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 8
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 1865
- Timestamp: 10:52:33:962_0
- RFN: 3389
- Chip: 22528
- Event: Timeout
- Source: tc_7_2_3_19:lt_TxAndRx LINE 6
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 1888
- Timestamp: 10:52:34:040_0
- RFN: 3397
- Chip: 17152
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000000'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000110'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001000'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'FFE665A5C5CA3452085408'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 01 05 09 0d 11 14 ff e6 65 a5 c5 ca 34 52 08 54 08

- No.: 1897
- Timestamp: 10:52:34:053_1
- RFN: 3398
- Chip: 31488
- Event: Start Timer
- Source: tc_7_2_3_19:lt_TxAndRx LINE 10
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 1898
- Timestamp: 10:52:34:054_0
- RFN: 3398
- Chip: 33280
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1903
- Timestamp: 10:52:34:062_0
- RFN: 3399
- Chip: 24320
- Event: Timeout
- Source: tc_7_2_3_19:lt_TxAndRx LINE 6
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 1905
- Timestamp: 10:52:34:065_0
- RFN: 3399
- Chip: 35584
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1910
- Timestamp: 10:52:34:213_0
- RFN: 3414
- Chip: 28160
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000000'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110011'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110011'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111001101111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111001101111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111001101111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'E6FFE6FFE6'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 00 ff e6 ff e6 ff e6 ff e6 ff e6 ff e6 ff e6 ff e6

- No.: 1914
- Timestamp: 10:52:34:219_1
- RFN: 3415
- Chip: 11776
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1919
- Timestamp: 10:52:34:233_0
- RFN: 3416
- Chip: 28928
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000001'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110011'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110011'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111001101111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111001101111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111001101111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'E6FFE6FFE6'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 08 ff e6 ff e6 ff e6 ff e6 ff e6 ff e6 ff e6 ff e6

- No.: 1923
- Timestamp: 10:52:34:239_2
- RFN: 3417
- Chip: 12288
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1928
- Timestamp: 10:52:34:253_0
- RFN: 3418
- Chip: 28928
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000010'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110011'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110011'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111001101111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111001101111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111001101111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'E6FFE6FFE6'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 10 ff e6 ff e6 ff e6 ff e6 ff e6 ff e6 ff e6 ff e6

- No.: 1932
- Timestamp: 10:52:34:259_1
- RFN: 3419
- Chip: 12288
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1937
- Timestamp: 10:52:34:273_0
- RFN: 3420
- Chip: 29440
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000011'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110011'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110011'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111001101111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111001101111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111001101111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'E6FFE6FFE6'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 18 ff e6 ff e6 ff e6 ff e6 ff e6 ff e6 ff e6 ff e6

- No.: 1941
- Timestamp: 10:52:34:279_2
- RFN: 3421
- Chip: 13056
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1946
- Timestamp: 10:52:34:294_0
- RFN: 3422
- Chip: 30720
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000100'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110011'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110011'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111111111110011'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111111111110011'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111111111110011'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = 'FFE6FFE6FF'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 21 1e ff e6 ff e6 ff e6 ff e6 ff e6 ff e6 ff e6 ff

- No.: 1950
- Timestamp: 10:52:34:300_0
- RFN: 3423
- Chip: 15872
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1955
- Timestamp: 10:52:34:315_0
- RFN: 3424
- Chip: 36352
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000101'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101001010110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101001010110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101001010110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'A565A565A5'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 28 65 a5 65 a5 65 a5 65 a5 65 a5 65 a5 65 a5 65 a5

- No.: 1959
- Timestamp: 10:52:34:321_0
- RFN: 3425
- Chip: 20224
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1962
- Timestamp: 10:52:34:332_0
- RFN: 3426
- Chip: 26368
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000110'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101001010110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101001010110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101001010110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'A565A565A5'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 30 65 a5 65 a5 65 a5 65 a5 65 a5 65 a5 65 a5 65 a5

- No.: 1966
- Timestamp: 10:52:34:338_2
- RFN: 3427
- Chip: 9984
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1971
- Timestamp: 10:52:34:352_0
- RFN: 3428
- Chip: 26624
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000111'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101001010110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101001010110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101001010110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'A565A565A5'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 38 65 a5 65 a5 65 a5 65 a5 65 a5 65 a5 65 a5 65 a5

- No.: 1975
- Timestamp: 10:52:34:358_2
- RFN: 3429
- Chip: 10496
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1980
- Timestamp: 10:52:34:372_0
- RFN: 3430
- Chip: 26368
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000001000'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101001010110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101001010110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101001010110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'A565A565A5'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 40 65 a5 65 a5 65 a5 65 a5 65 a5 65 a5 65 a5 65 a5

- No.: 1984
- Timestamp: 10:52:34:378_3
- RFN: 3431
- Chip: 11264
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1989
- Timestamp: 10:52:34:394_0
- RFN: 3432
- Chip: 31744
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000001001'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '011001011010010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '011001011010010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '011001011010010'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = '65A565A565'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 49 1e 65 a5 65 a5 65 a5 65 a5 65 a5 65 a5 65 a5 65

- No.: 1993
- Timestamp: 10:52:34:400_3
- RFN: 3433
- Chip: 15360
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1998
- Timestamp: 10:52:34:415_0
- RFN: 3434
- Chip: 32256
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000001010'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100101'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100101'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110010101100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110010101100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110010101100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'CAC5CAC5CA'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 50 c5 ca c5 ca c5 ca c5 ca c5 ca c5 ca c5 ca c5 ca

- No.: 2002
- Timestamp: 10:52:34:420_3
- RFN: 3435
- Chip: 15872
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2007
- Timestamp: 10:52:34:435_0
- RFN: 3436
- Chip: 32768
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000001011'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100101'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100101'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110010101100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110010101100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110010101100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'CAC5CAC5CA'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 58 c5 ca c5 ca c5 ca c5 ca c5 ca c5 ca c5 ca c5 ca

- No.: 2011
- Timestamp: 10:52:34:440_3
- RFN: 3437
- Chip: 16896
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2016
- Timestamp: 10:52:34:455_0
- RFN: 3438
- Chip: 34816
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000001100'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100101'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100101'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110010101100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110010101100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110010101100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'CAC5CAC5CA'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 60 c5 ca c5 ca c5 ca c5 ca c5 ca c5 ca c5 ca c5 ca

- No.: 2020
- Timestamp: 10:52:34:461_2
- RFN: 3439
- Chip: 19968
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2025
- Timestamp: 10:52:34:476_0
- RFN: 3441
- Chip: 1792
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000001101'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100101'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100101'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110010101100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110010101100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110010101100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'CAC5CAC5CA'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 68 c5 ca c5 ca c5 ca c5 ca c5 ca c5 ca c5 ca c5 ca

- No.: 2029
- Timestamp: 10:52:34:485_0
- RFN: 3441
- Chip: 33024
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2032
- Timestamp: 10:52:34:494_0
- RFN: 3442
- Chip: 31744
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000001110'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100101'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100101'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110001011100101'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110001011100101'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110001011100101'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = 'C5CAC5CAC5'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 71 1e c5 ca c5 ca c5 ca c5 ca c5 ca c5 ca c5 ca c5

- No.: 2036
- Timestamp: 10:52:34:500_1
- RFN: 3443
- Chip: 15104
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2041
- Timestamp: 10:52:34:514_0
- RFN: 3444
- Chip: 32000
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000001111'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101001'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101001'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010100100011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010100100011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010100100011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '5234523452'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 78 34 52 34 52 34 52 34 52 34 52 34 52 34 52 34 52

- No.: 2045
- Timestamp: 10:52:34:520_3
- RFN: 3445
- Chip: 16640
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2050
- Timestamp: 10:52:34:535_0
- RFN: 3446
- Chip: 36608
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000010000'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101001'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101001'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010100100011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010100100011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010100100011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '5234523452'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 80 34 52 34 52 34 52 34 52 34 52 34 52 34 52 34 52

- No.: 2054
- Timestamp: 10:52:34:541_2
- RFN: 3447
- Chip: 20736
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2057
- Timestamp: 10:52:34:553_0
- RFN: 3448
- Chip: 27392
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000010001'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101001'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101001'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010100100011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010100100011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010100100011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '5234523452'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 8c 34 52 34 52 34 52 34 52 34 52 34 52 34 52 34 52

- No.: 2063
- Timestamp: 10:52:34:569_1
- RFN: 3450
- Chip: 13056
- Event: Start Timer
- Source: tc_7_2_3_19:lt_CheckPollBit LINE 5
- Message Structure:
no details available
- Constraint:
t_LowerBound (405 Ms)
- BinaryMessage:

- No.: 2064
- Timestamp: 10:52:34:570_0
- RFN: 3450
- Chip: 14592
- Event: Start Timer
- Source: tc_7_2_3_19:lt_CheckPollBit LINE 5
- Message Structure:
no details available
- Constraint:
t_UpperBound (595 Ms)
- BinaryMessage:

- No.: 2066
- Timestamp: 10:52:34:570_2
- RFN: 3450
- Chip: 16384
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2069
- Timestamp: 10:52:34:580_0
- RFN: 3451
- Chip: 16640
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000010010'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101001'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101001'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010100100011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010100100011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010100100011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '5234523452'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 90 34 52 34 52 34 52 34 52 34 52 34 52 34 52 34 52

- No.: 2073
- Timestamp: 10:52:34:588_3
- RFN: 3452
- Chip: 9984
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2076
- Timestamp: 10:52:34:598_0
- RFN: 3453
- Chip: 8704
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000010011'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101001'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101001'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '001101000101001'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '001101000101001'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '001101000101001'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '3452345234'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 99 1e 34 52 34 52 34 52 34 52 34 52 34 52 34 52 34

- No.: 2080
- Timestamp: 10:52:34:606_2
- RFN: 3454
- Chip: 1536
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2083
- Timestamp: 10:52:34:616_0
- RFN: 3455
- Chip: 1792
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000010100'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010101000000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010101000000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010101000000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '5408540854'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 a0 08 54 08 54 08 54 08 54 08 54 08 54 08 54 08 54

- No.: 2087
- Timestamp: 10:52:34:624_2
- RFN: 3455
- Chip: 32768
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2090
- Timestamp: 10:52:34:634_0
- RFN: 3456
- Chip: 32256
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000010101'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010101000000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010101000000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010101000000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '5408540854'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 a8 08 54 08 54 08 54 08 54 08 54 08 54 08 54 08 54

- No.: 2094
- Timestamp: 10:52:34:640_0
- RFN: 3457
- Chip: 15616
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2099
- Timestamp: 10:52:34:654_0
- RFN: 3458
- Chip: 32256
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000010110'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010101000000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010101000000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010101000000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '5408540854'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 b0 08 54 08 54 08 54 08 54 08 54 08 54 08 54 08 54

- No.: 2103
- Timestamp: 10:52:34:660_2
- RFN: 3459
- Chip: 18688
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2108
- Timestamp: 10:52:34:675_0
- RFN: 3461
- Chip: 0
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000010111'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010101000000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010101000000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010101000000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '5408540854'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 b8 08 54 08 54 08 54 08 54 08 54 08 54 08 54 08 54

- No.: 2112
- Timestamp: 10:52:34:682_0
- RFN: 3461
- Chip: 24832
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2117
- Timestamp: 10:52:34:696_0
- RFN: 3463
- Chip: 4096
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000011000'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '000010000101010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '000010000101010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '000010000101010'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '0854085408'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 c1 1e 08 54 08 54 08 54 08 54 08 54 08 54 08 54 08

- No.: 2121
- Timestamp: 10:52:34:703_3
- RFN: 3463
- Chip: 27136
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2126
- Timestamp: 10:52:34:971_1
- RFN: 3490
- Chip: 22784
- Event: Timeout
- Source: tc_7_2_3_19:lt_TxAndRx LINE 1
- Message Structure:
no details available
- Constraint:
t_LowerBound
- BinaryMessage:

- No.: 2128
- Timestamp: 10:52:34:974_1
- RFN: 3490
- Chip: 34048
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2133
- Timestamp: 10:52:35:053_0
- RFN: 3498
- Chip: 28160
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000011000'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '000010000101010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '000010000101010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '000010000101010'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '0854085408'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 c5 1e 08 54 08 54 08 54 08 54 08 54 08 54 08 54 08

- No.: 2139
- Timestamp: 10:52:35:067_1
- RFN: 3500
- Chip: 4352
- Event: Start Timer
- Source: tc_7_2_3_19:lt_CheckPollBit LINE 7
- Message Structure:
no details available
- Constraint:
t_Dly (5000 Ms)
- BinaryMessage:

- No.: 2141
- Timestamp: 10:52:35:071_0
- RFN: 3500
- Chip: 16896
- Event: Cancel Timer
- Source: tc_7_2_3_19:lt_CheckPollBit LINE 8
- Message Structure:
no details available
- Constraint:
t_UpperBound
- BinaryMessage:

- No.: 2142
- Timestamp: 10:52:35:086_0
- RFN: 3501
- Chip: 38144
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: tc_7_2_3_19:lt_CheckPollBit LINE 9
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. STATUS_PDU
. . (DC_Field)dC_Field[1] = '0'B
. . (CtrlPDU_Type)type[3] = '000'B
. . SuperFields
. . . SUFI_WindowSize
. . . SUFI_List
. . . SUFI_RList
. . . SUFI_Bitmap
. . . SUFI_MRW
. . . SUFI_MRW_ACK
. . . SUFI_NoMore
. . . SUFI_Ack
. . . . (SUFI_Type)type[4] = '0010'B
. . . . (AM_SeqNum)lsn[12] = '000000011001'B
. . (HexStringType)superFieldsAndPadRx[-1] = -
. . (Padding)paddingTx[-1] = '0000000000000000000000000000000'H
- Constraint:
cas_StatusReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 02 01 90 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00

- No.: 2146
- Timestamp: 10:52:35:091_0
- RFN: 3502
- Chip: 17408
- Event: Start Timer
- Source: tc_7_2_3_19:lt_MonitorUplink LINE 1
- Message Structure:
no details available
- Constraint:
t_WaitMS (1000 Ms)
- BinaryMessage:

- No.: 2150
- Timestamp: 10:52:36:090_0
- RFN: 3602
- Chip: 17408
- Event: Timeout
- Source: tc_7_2_3_19:lt_MonitorUplink LINE 3
- Message Structure:
no details available
- Constraint:
t_WaitMS
- BinaryMessage:

- No.: 2153
- Timestamp: 10:52:36:094_0
- RFN: 3602
- Chip: 29952
- Event: Start Timer
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 11
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 2160
- Timestamp: 10:52:36:115_0
- RFN: 3604
- Chip: 33792
- Event: Timeout
- Source: tc_7_2_3_19:lt_TxAndRx LINE 6
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 2183
- Timestamp: 10:52:36:163_0
- RFN: 3609
- Chip: 28416
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000001'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000110'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001000'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'ABEECE4B0B813FD337873F'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 09 05 09 0d 11 14 ab ee ce 4b 0b 81 3f d3 37 87 3f

- No.: 2192
- Timestamp: 10:52:36:178_1
- RFN: 3611
- Chip: 11008
- Event: Start Timer
- Source: tc_7_2_3_19:lt_TxAndRx LINE 10
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 2193
- Timestamp: 10:52:36:179_0
- RFN: 3611
- Chip: 12032
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2198
- Timestamp: 10:52:36:203_0
- RFN: 3613
- Chip: 27904
- Event: Timeout
- Source: tc_7_2_3_19:lt_TxAndRx LINE 6
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 2200
- Timestamp: 10:52:36:206_1
- RFN: 3614
- Chip: 1280
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2205
- Timestamp: 10:52:36:334_0
- RFN: 3626
- Chip: 29696
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000011001'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111011100000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101010111110111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '000010001010101'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'EE08ABEE08'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 c8 08 ab ee 08 ab ee 08 ab ee 08 ab ee 08 ab ee 08

- No.: 2209
- Timestamp: 10:52:36:340_0
- RFN: 3627
- Chip: 13568
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2214
- Timestamp: 10:52:36:354_0
- RFN: 3628
- Chip: 29952
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000011010'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '000010001010101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111011100000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101010111110111'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '08ABEE08AB'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 d0 ab ee 08 ab ee 08 ab ee 08 ab ee 08 ab ee 08 ab

- No.: 2218
- Timestamp: 10:52:36:360_0
- RFN: 3629
- Chip: 14080
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2223
- Timestamp: 10:52:36:374_0
- RFN: 3630
- Chip: 30720
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000011011'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101010111110111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '000010001010101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111011100000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = 'ABEE08ABEE'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 d8 ee 08 ab ee 08 ab ee 08 ab ee 08 ab ee 08 ab ee

- No.: 2227
- Timestamp: 10:52:36:380_2
- RFN: 3631
- Chip: 15360
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2232
- Timestamp: 10:52:36:394_0
- RFN: 3632
- Chip: 33024
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000011100'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111011100000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101010111110111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '000010001010101'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'EE08ABEE08'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 e0 08 ab ee 08 ab ee 08 ab ee 08 ab ee 08 ab ee 08

- No.: 2236
- Timestamp: 10:52:36:400_3
- RFN: 3633
- Chip: 16384
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2241
- Timestamp: 10:52:36:415_0
- RFN: 3634
- Chip: 33536
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000011101'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111011100000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101010111110111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '000010001010101'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'EE08ABEE08'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 e9 1e ab ee 08 ab ee 08 ab ee 08 ab ee 08 ab ee 08

- No.: 2245
- Timestamp: 10:52:36:420_3
- RFN: 3635
- Chip: 17152
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2250
- Timestamp: 10:52:36:435_0
- RFN: 3636
- Chip: 34048
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000011110'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0100101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0100101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010010111100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010010111100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010010111100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '4BCE4BCE4B'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 f0 ce 4b ce 4b ce 4b ce 4b ce 4b ce 4b ce 4b ce 4b

- No.: 2254
- Timestamp: 10:52:36:440_3
- RFN: 3637
- Chip: 17664
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2259
- Timestamp: 10:52:36:455_0
- RFN: 3638
- Chip: 34304
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000011111'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0100101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0100101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010010111100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010010111100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010010111100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '4BCE4BCE4B'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 f8 ce 4b ce 4b ce 4b ce 4b ce 4b ce 4b ce 4b ce 4b

- No.: 2263
- Timestamp: 10:52:36:460_3
- RFN: 3639
- Chip: 17920
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2268
- Timestamp: 10:52:36:475_0
- RFN: 3640
- Chip: 34560
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000100000'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0100101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0100101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010010111100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010010111100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010010111100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '4BCE4BCE4B'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 00 ce 4b ce 4b ce 4b ce 4b ce 4b ce 4b ce 4b ce 4b

- No.: 2272
- Timestamp: 10:52:36:480_3
- RFN: 3641
- Chip: 17664
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2277
- Timestamp: 10:52:36:495_0
- RFN: 3642
- Chip: 34560
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000100001'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0100101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0100101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010010111100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010010111100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010010111100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '4BCE4BCE4B'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 08 ce 4b ce 4b ce 4b ce 4b ce 4b ce 4b ce 4b ce 4b

- No.: 2281
- Timestamp: 10:52:36:500_3
- RFN: 3643
- Chip: 17920
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2286
- Timestamp: 10:52:36:514_0
- RFN: 3644
- Chip: 34304
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000100010'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0100101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0100101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110011100100101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110011100100101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110011100100101'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'CE4BCE4BCE'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 11 1e ce 4b ce 4b ce 4b ce 4b ce 4b ce 4b ce 4b ce

- No.: 2290
- Timestamp: 10:52:36:520_2
- RFN: 3645
- Chip: 17920
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2295
- Timestamp: 10:52:36:534_0
- RFN: 3646
- Chip: 34048
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000100011'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000000'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000000'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100000010000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100000010000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100000010000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = '810B810B81'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 18 0b 81 0b 81 0b 81 0b 81 0b 81 0b 81 0b 81 0b 81

- No.: 2299
- Timestamp: 10:52:36:540_3
- RFN: 3647
- Chip: 18176
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2304
- Timestamp: 10:52:36:554_0
- RFN: 3648
- Chip: 34816
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000100100'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000000'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000000'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100000010000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100000010000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100000010000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = '810B810B81'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 24 0b 81 0b 81 0b 81 0b 81 0b 81 0b 81 0b 81 0b 81

- No.: 2311
- Timestamp: 10:52:36:571_2
- RFN: 3650
- Chip: 22528
- Event: Read Timer
- Source: tc_7_2_3_19:lt_CheckTimeDiff LINE 1
- Message Structure:
no details available
- Constraint:
t_Dly (1500 ÌÌÌÌÌÌÌÌ)
- BinaryMessage:

- No.: 2313
- Timestamp: 10:52:36:574_1
- RFN: 3650
- Chip: 34560
- Event: Cancel Timer
- Source: tc_7_2_3_19:lt_CheckTimeDiff LINE 2
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 2317
- Timestamp: 10:52:36:579_1
- RFN: 3651
- Chip: 9984
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2320
- Timestamp: 10:52:36:590_0
- RFN: 3652
- Chip: 13824
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000100101'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000000'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000000'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100000010000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100000010000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100000010000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = '810B810B81'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 28 0b 81 0b 81 0b 81 0b 81 0b 81 0b 81 0b 81 0b 81

- No.: 2324
- Timestamp: 10:52:36:597_3
- RFN: 3653
- Chip: 3840
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2327
- Timestamp: 10:52:36:610_0
- RFN: 3654
- Chip: 13056
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000100110'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000000'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000000'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100000010000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100000010000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100000010000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = '810B810B81'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 30 0b 81 0b 81 0b 81 0b 81 0b 81 0b 81 0b 81 0b 81

- No.: 2331
- Timestamp: 10:52:36:616_1
- RFN: 3654
- Chip: 36864
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2334
- Timestamp: 10:52:36:627_0
- RFN: 3656
- Chip: 3584
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000100111'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000000'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000000'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '000010111000000'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '000010111000000'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '000010111000000'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = '0B810B810B'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 39 1e 0b 81 0b 81 0b 81 0b 81 0b 81 0b 81 0b 81 0b

- No.: 2338
- Timestamp: 10:52:36:633_2
- RFN: 3656
- Chip: 26880
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2341
- Timestamp: 10:52:36:644_0
- RFN: 3657
- Chip: 31744
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000101000'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1101001'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1101001'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110100110011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110100110011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110100110011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'D33FD33FD3'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 40 3f d3 3f d3 3f d3 3f d3 3f d3 3f d3 3f d3 3f d3

- No.: 2345
- Timestamp: 10:52:36:650_3
- RFN: 3658
- Chip: 16896
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2348
- Timestamp: 10:52:36:660_0
- RFN: 3659
- Chip: 13568
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000101001'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1101001'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1101001'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110100110011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110100110011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110100110011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'D33FD33FD3'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 48 3f d3 3f d3 3f d3 3f d3 3f d3 3f d3 3f d3 3f d3

- No.: 2352
- Timestamp: 10:52:36:668_1
- RFN: 3660
- Chip: 7168
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2355
- Timestamp: 10:52:36:678_0
- RFN: 3661
- Chip: 5888
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000101010'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1101001'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1101001'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110100110011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110100110011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110100110011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'D33FD33FD3'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 50 3f d3 3f d3 3f d3 3f d3 3f d3 3f d3 3f d3 3f d3

- No.: 2359
- Timestamp: 10:52:36:684_1
- RFN: 3661
- Chip: 29952
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2364
- Timestamp: 10:52:36:699_0
- RFN: 3663
- Chip: 11264
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000101011'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1101001'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1101001'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110100110011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110100110011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110100110011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'D33FD33FD3'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 58 3f d3 3f d3 3f d3 3f d3 3f d3 3f d3 3f d3 3f d3

- No.: 2368
- Timestamp: 10:52:36:707_2
- RFN: 3664
- Chip: 4608
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2371
- Timestamp: 10:52:36:717_0
- RFN: 3665
- Chip: 3584
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000101100'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1101001'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1101001'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '001111111101001'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '001111111101001'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '001111111101001'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = '3FD33FD33F'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 61 1e 3f d3 3f d3 3f d3 3f d3 3f d3 3f d3 3f d3 3f

- No.: 2375
- Timestamp: 10:52:36:723_3
- RFN: 3665
- Chip: 28160
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2380
- Timestamp: 10:52:36:737_0
- RFN: 3667
- Chip: 4864
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000101101'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100001110011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100001110011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100001110011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = '8737873787'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 68 37 87 37 87 37 87 37 87 37 87 37 87 37 87 37 87

- No.: 2384
- Timestamp: 10:52:36:745_2
- RFN: 3667
- Chip: 35840
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2387
- Timestamp: 10:52:36:755_0
- RFN: 3668
- Chip: 34304
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000101110'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100001110011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100001110011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100001110011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = '8737873787'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 70 37 87 37 87 37 87 37 87 37 87 37 87 37 87 37 87

- No.: 2391
- Timestamp: 10:52:36:761_1
- RFN: 3669
- Chip: 19456
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2396
- Timestamp: 10:52:36:776_0
- RFN: 3671
- Chip: 3328
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000101111'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100001110011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100001110011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100001110011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = '8737873787'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 78 37 87 37 87 37 87 37 87 37 87 37 87 37 87 37 87

- No.: 2400
- Timestamp: 10:52:36:783_1
- RFN: 3671
- Chip: 27648
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2405
- Timestamp: 10:52:36:797_0
- RFN: 3673
- Chip: 4096
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000110000'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100001110011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100001110011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100001110011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = '8737873787'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 80 37 87 37 87 37 87 37 87 37 87 37 87 37 87 37 87

- No.: 2409
- Timestamp: 10:52:36:805_1
- RFN: 3673
- Chip: 35072
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2412
- Timestamp: 10:52:36:814_0
- RFN: 3674
- Chip: 33536
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000110001'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '001101111000011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '001101111000011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '001101111000011'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = '3787378737'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 89 1e 37 87 37 87 37 87 37 87 37 87 37 87 37 87 37

- No.: 2423
- Timestamp: 10:52:37:053_0
- RFN: 3698
- Chip: 28928
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000110001'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '001101111000011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '001101111000011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '001101111000011'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = '3787378737'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 8d 1e 37 87 37 87 37 87 37 87 37 87 37 87 37 87 37

- No.: 2431
- Timestamp: 10:52:37:067_2
- RFN: 3700
- Chip: 6400
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: tc_7_2_3_19:lt_CheckNumPolls LINE 1
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2432
- Timestamp: 10:52:37:074_0
- RFN: 3700
- Chip: 30720
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: tc_7_2_3_19:lt_CheckNumPolls LINE 2
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. STATUS_PDU
. . (DC_Field)dC_Field[1] = '0'B
. . (CtrlPDU_Type)type[3] = '000'B
. . SuperFields
. . . SUFI_WindowSize
. . . SUFI_List
. . . SUFI_RList
. . . SUFI_Bitmap
. . . SUFI_MRW
. . . SUFI_MRW_ACK
. . . SUFI_NoMore
. . . SUFI_Ack
. . . . (SUFI_Type)type[4] = '0010'B
. . . . (AM_SeqNum)lsn[12] = '000000110010'B
. . (HexStringType)superFieldsAndPadRx[-1] = -
. . (Padding)paddingTx[-1] = '0000000000000000000000000000000'H
- Constraint:
cas_StatusReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 02 03 20 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00

- No.: 2438
- Timestamp: 10:52:37:086_0
- RFN: 3701
- Chip: 37888
- Event: Send
- PCO: Dc
- Message: RRC_DataReq
- Source: ts_TC_OpenUE_TestLoop LINE 6
- Message Structure:
RRC_DataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[-1] = -
. (SapId)sapId[1] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. OPENUETESTLOOP
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)tCProtocolDiscriminator[4] = '1111'B
. . (MsgType)msgType[8] = '01000010'B
- Constraint:
ca_PS_DataReq
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 0f 42

- No.: 2439
- Timestamp: 10:52:37:086_1
- RFN: 3702
- Chip: 3072
- Event: Start Timer
- Source: ts_TC_OpenUE_TestLoop LINE 6
- Message Structure:
no details available
- Constraint:
t_Dly (5000 Ms)
- BinaryMessage:

- No.: 2443
- Timestamp: 10:52:37:369_0
- RFN: 3730
- Chip: 12032
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_TC_OpenUE_TestLoop LINE 7
- Message Structure:
RRC_DataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. (START_Value)start[0] = -
. OPENUETESTLOOPCOMPLETE
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)tCProtocolDiscriminator[4] = '1111'B
. . (MsgType)msgType[8] = '01000011'B
- Constraint:
car_PS_UplinkDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 0f 43

- No.: 2444
- Timestamp: 10:52:37:370_0
- RFN: 3730
- Chip: 15360
- Event: Cancel Timer
- Source: ts_TC_OpenUE_TestLoop LINE 7
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 2445
- Timestamp: 10:52:37:370_1
- RFN: 3730
- Chip: 16128
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_TC_OpenUE_TestLoop LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2463
- Timestamp: 10:52:37:388_0
- RFN: 3732
- Chip: 9984
- Event: Send
- PCO: CPHY
- Message: CPHY_Frame_Number_REQ
- Source: ts_CPHY_ActTime LINE 1
- Message Structure:
CPHY_Frame_Number_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
cas_GetFrameNum
- BinaryMessage:
30 06 02 01 00 02 01 1a

- No.: 2467
- Timestamp: 10:52:37:396_0
- RFN: 3732
- Chip: 37632
- Event: Receive
- PCO: CPHY
- Message: CPHY_Frame_Number_CNF
- Source: ts_CPHY_ActTime LINE 2
- Message Structure:
CPHY_Frame_Number_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
. (IntegerType)frameNumber = 148
- Constraint:
car_GetFrameNum
- BinaryMessage:
30 0a 02 01 00 02 01 1a 02 02 00 94

- No.: 2473
- Timestamp: 10:52:37:450_0
- RFN: 3738
- Chip: 16128
- Event: Send
- PCO: AM
- Message: RLC_AM_DATA_REQ
- Source: ts_RRC_RB_RelRLC:lt_SendRAB_Rel LINE 4
- Message Structure:
RLC_AM_DATA_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. AmConfirmationRequest
. aM_message
. . DL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00000000000000000000000000000000"
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . DL_DCCH_MessageType
. . . . RadioBearerRelease
. . . . . r3
. . . . . . RadioBearerRelease_r3_IEs
. . . . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . . . IntegrityProtectionModeInfo
. . . . . . . CipheringModeInfo
. . . . . . . (IntegerType)activationTime = 136
. . . . . . . U_RNTI
. . . . . . . (BitStringType)new_C_RNTI[16] = -
. . . . . . . (RRC_StateIndicator)rrc_StateIndicator = 0
. . . . . . . (IntegerType)utran_DRX_CycleLengthCoeff = -
. . . . . . . CN_InformationInfo
. . . . . . . (CN_DomainIdentity)signallingConnectionRelIndication = -
. . . . . . . (BitStringType)ura_Identity[16] = -
. . . . . . . RAB_InformationReconfigList
. . . . . . . RB_InformationReleaseList
. . . . . . . . (IntegerType)_elem = 20
. . . . . . . RB_InformationAffectedList
. . . . . . . DL_CounterSynchronisationInfo
. . . . . . . UL_CommonTransChInfo
. . . . . . . . TFC_Subset
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . TFCS
. . . . . . . . . . . ExplicitTFCS_Configuration
. . . . . . . . . . . . TFCS_ReconfAdd
. . . . . . . . . . . . . ctfcSize
. . . . . . . . . . . . . . ctfc2Bit
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . . . . . . . (IntegerType)ctfc2 = 0
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . . . . . . . (IntegerType)ctfc2 = 1
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 11
. . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . UL_DeletedTransChInfoList
. . . . . . . . UL_TransportChannelIdentity
. . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType = 0
. . . . . . . . . (IntegerType)ul_TransportChannelIdentity = 1
. . . . . . . UL_AddReconfTransChInfoList
. . . . . . . . UL_AddReconfTransChInformation
. . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType = 0
. . . . . . . . . (IntegerType)transportChannelIdentity = 5
. . . . . . . . . TransportFormatSet
. . . . . . . . . . DedicatedTransChTFS
. . . . . . . . . . . tti
. . . . . . . . . . . . DedicatedDynamicTF_InfoList
. . . . . . . . . . . . . DedicatedDynamicTF_Info
. . . . . . . . . . . . . . rlc_Size
. . . . . . . . . . . . . . . BitModeRLC_SizeInfo
. . . . . . . . . . . . . . . . sizeType2
. . . . . . . . . . . . . . . . . (IntegerType)part1 = 2
. . . . . . . . . . . . . . . . . (IntegerType)part2 = -
. . . . . . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . LogicalChannelList
. . . . . . . . . . . SemistaticTF_Information
. . . . . . . . . . . . ChannelCodingType
. . . . . . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . . . . . (IntegerType)rateMatchingAttribute = 192
. . . . . . . . . . . . (CRC_Size)crc_Size = 3
. . . . . . . modeSpecificTransChInfo
. . . . . . . . fdd
. . . . . . . . . (IntegerType)cpch_SetID = -
. . . . . . . . . DRAC_StaticInformationList
. . . . . . . DL_CommonTransChInfo
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . dl_Parameters
. . . . . . . DL_DeletedTransChInfoList
. . . . . . . . DL_TransportChannelIdentity
. . . . . . . . . (DL_TrCH_Type)dl_TransportChannelType = 0
. . . . . . . . . (IntegerType)dl_TransportChannelIdentity = 6
. . . . . . . DL_AddReconfTransChInfo2List
. . . . . . . . DL_AddReconfTransChInformation2
. . . . . . . . . (DL_TrCH_Type)dl_TransportChannelType = 0
. . . . . . . . . (IntegerType)transportChannelIdentity = 10
. . . . . . . . . tfs_SignallingMode
. . . . . . . . . . UL_TransportChannelIdentity
. . . . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType = 0
. . . . . . . . . . . (IntegerType)ul_TransportChannelIdentity = 5
. . . . . . . . . QualityTarget
. . . . . . . FrequencyInfo
. . . . . . . . modeSpecificInfo
. . . . . . . . . FrequencyInfoFDD
. . . . . . . . . . (IntegerType)uarfcn_UL = -
. . . . . . . . . . (IntegerType)uarfcn_DL = 10700
. . . . . . . (IntegerType)maxAllowedUL_TX_Power = 33
. . . . . . . UL_ChannelRequirement
. . . . . . . . UL_DPCH_Info
. . . . . . . . . UL_DPCH_PowerControlInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (IntegerType)dpcch_PowerOffset = -40
. . . . . . . . . . . (IntegerType)pc_Preamble = 1
. . . . . . . . . . . (IntegerType)sRB_delay = 7
. . . . . . . . . . . PowerControlAlgorithm
. . . . . . . . . . . . (IntegerType)algorithm1 = 1
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (ScramblingCodeType)scramblingCodeType = 1
. . . . . . . . . . . (IntegerType)scramblingCode = 0
. . . . . . . . . . . (IntegerType)numberOfDPDCH = -
. . . . . . . . . . . (SpreadingFactor)spreadingFactor = 4
. . . . . . . . . . . (BooleanType)tfci_Existence = TRUE
. . . . . . . . . . . (IntegerType)numberOfFBI_Bits = -
. . . . . . . . . . . (PuncturingLimit)puncturingLimit = 15
. . . . . . . modeSpecificPhysChInfo
. . . . . . . . fdd
. . . . . . . . . DL_PDSCH_Information
. . . . . . . DL_CommonInformation
. . . . . . . . DL_DPCH_InfoCommon
. . . . . . . . . cfnHandling
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . DL_DPCH_PowerControlInfo
. . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . (DPC_Mode)dpc_Mode = 0
. . . . . . . . . . . (IntegerType)powerOffsetPilot_pdpdch = 0
. . . . . . . . . . . Dl_rate_matching_restriction
. . . . . . . . . . . SF512_AndPilot
. . . . . . . . . . . . (PilotBits128)sfd128 = 0
. . . . . . . . . . . (PositionFixedOrFlexible)positionFixedOrFlexible = 0
. . . . . . . . . . . (BooleanType)tfci_Existence = FALSE
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . (IntegerType)defaultDPCH_OffsetValue = -
. . . . . . . . . . DPCH_CompressedModeInfo
. . . . . . . . . . (TX_DiversityMode)tx_DiversityMode = 0
. . . . . . . . . . SSDT_Information
. . . . . . . DL_InformationPerRL_List
. . . . . . . . DL_InformationPerRL
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . PrimaryCPICH_Info
. . . . . . . . . . . . (IntegerType)primaryScramblingCode = 100
. . . . . . . . . . . PDSCH_SHO_DCH_Info
. . . . . . . . . . . PDSCH_CodeMapping
. . . . . . . . . DL_DPCH_InfoPerRL
. . . . . . . . . . fdd
. . . . . . . . . . . (PCPICH_UsageForChannelEst)pCPICH_UsageForChannelEst = 0
. . . . . . . . . . . (IntegerType)dpch_FrameOffset = 0
. . . . . . . . . . . SecondaryCPICH_Info
. . . . . . . . . . . DL_ChannelisationCodeList
. . . . . . . . . . . . DL_ChannelisationCode
. . . . . . . . . . . . . (IntegerType)secondaryScramblingCode = 1
. . . . . . . . . . . . . SF512_AndCodeNumber
. . . . . . . . . . . . . . (IntegerType)sf128 = 0
. . . . . . . . . . . . . (ScramblingCodeChange)scramblingCodeChange = -
. . . . . . . . . . . (IntegerType)tpc_CombinationIndex = 0
. . . . . . . . . . . (SSDT_CellIdentity)ssdt_CellIdentity = -
. . . . . . . . . . . (ClosedLoopTimingAdjMode)closedLoopTimingAdjMode = -
. . . . . . . . . SCCPCH_InfoForFACH
. . . . . . v3a0NonCriticalExtensions
. . . . . . . RadioBearerRelease_v3a0ext
. . . . . . . . (BitStringType)new_DSCH_RNTI[16] = -
. . . . . . . laterNonCriticalExtensions
- Constraint:
cas_RB_Release
- BinaryMessage:
30 3a 02 01 ff 02 01 02 05 00 80 00 00 00 03 52 00 ff f2 20 04 c8 00 06 25 2b f0 00 00 40 01 10 44 77 ec 18 05 00 98 85 39 94 d2 a3 d1 00 00 00 9f 24 02 81 02 06 40 00 08 28 00 00

- No.: 2484
- Timestamp: 10:52:37:467_0
- RFN: 3740
- Chip: 7424
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = -12
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 f4 0a 01 00 05 00

- No.: 2488
- Timestamp: 10:52:37:476_0
- RFN: 3741
- Chip: 2048
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = -12
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 f4

- No.: 2497
- Timestamp: 10:52:37:488_0
- RFN: 3742
- Chip: 10240
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Modify_REQ
- Source: ts_SS_1DCH_DCCH_Modify LINE 4
- Message Structure:
CPHY_RL_Modify_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
. (RatType)ratType = 0
. CphyRlModifyReq
. . SS_ActivationTime
. . . (IntegerType)activationCFN = 136
. . physicalChannelInfo
. . . DPCHInfo
. . . . UL_DPCH_Info
. . . . DL_DPCHInfo
. . . . . DL_CommonInformation
. . . . . . DL_DPCH_InfoCommon
. . . . . . . cfnHandling
. . . . . . . . initialise
. . . . . . . . . (IntegerType)cfntargetsfnframeoffset = -
. . . . . . . modeSpecificInfo
. . . . . . . . fdd
. . . . . . . . . DL_DPCH_PowerControlInfo
. . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . fdd
. . . . . . . . . . . . (DPC_Mode)dpc_Mode = 0
. . . . . . . . . (IntegerType)powerOffsetPilot_pdpdch = 0
. . . . . . . . . Dl_rate_matching_restriction
. . . . . . . . . SF512_AndPilot
. . . . . . . . . . (PilotBits128)sfd128 = 0
. . . . . . . . . (PositionFixedOrFlexible)positionFixedOrFlexible = 0
. . . . . . . . . (BooleanType)tfci_Existence = FALSE
. . . . . . modeSpecificInfo
. . . . . . . fdd
. . . . . . . . (IntegerType)defaultDPCH_OffsetValue = 0
. . . . . . . . DPCH_CompressedModeInfo
. . . . . . . . (TX_DiversityMode)tx_DiversityMode = 0
. . . . . . . . SSDT_Information
. . . . . DL_DPCH_InfoPerRL
. . . . . . fdd
. . . . . . . (PCPICH_UsageForChannelEst)pCPICH_UsageForChannelEst = 0
. . . . . . . (IntegerType)dpch_FrameOffset = 0
. . . . . . . SecondaryCPICH_Info
. . . . . . . DL_ChannelisationCodeList
. . . . . . . . DL_ChannelisationCode
. . . . . . . . . (IntegerType)secondaryScramblingCode = 1
. . . . . . . . . SF512_AndCodeNumber
. . . . . . . . . . (IntegerType)sf128 = 0
. . . . . . . . . (ScramblingCodeChange)scramblingCodeChange = -
. . . . . . . (IntegerType)tpc_CombinationIndex = 0
. . . . . . . (SSDT_CellIdentity)ssdt_CellIdentity = -
. . . . . . . (ClosedLoopTimingAdjMode)closedLoopTimingAdjMode = -
. . . . . (IntegerType)powerOffsetOfTFCI_PO1 = 0
. . . . . (IntegerType)powerOffsetOfTPC_PO2 = 0
. . . . . (IntegerType)powerOffsetOfPILOT_PO3 = 0
. . . . . (IntegerType)dl_TxPower = -5
. . . . . (IntegerType)dl_TxPowerMax = 15
. . . . . (IntegerType)dl_TxPowerMin = -35
- Constraint:
ca_DL_DPCH_ModifyInfo
- BinaryMessage:
30 62 02 01 00 02 01 1a 0a 01 00 30 57 02 02 00 88 30 51 30 4f 30 25 30 1a 30 30 00 30 30 14 30 06 30 30 03 0a 01 00 02 01 00 0a 01 00 0a 01 00 01 01 00 30 30 06 02 01 00 0a 01 00 30 30 13 0a 01 00 02 01 00 30 08 30 06 02 01 01 02 01 00 02 01 00 02 01 00 02 01 00 02 01 00 02 01 fb 02 01 0f 02 01 dd

- No.: 2501
- Timestamp: 10:52:37:495_0
- RFN: 3742
- Chip: 36608
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Modify_CNF
- Source: ts_SS_1DCH_DCCH_Modify LINE 5
- Message Structure:
CPHY_RL_Modify_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
ca_RL_ModifyCnf
- BinaryMessage:
30 06 02 01 00 02 01 1a

- No.: 2502
- Timestamp: 10:52:37:506_0
- RFN: 3744
- Chip: 2304
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Config_REQ
- Source: ts_SS_1DCH_DCCH_Modify LINE 6
- Message Structure:
CPHY_TrCH_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
. (RatType)ratType = 0
. CphyTrchConfigReq
. . SS_ActivationTime
. . . (IntegerType)activationCFN = 136
. . ulconnectedTrCHList
. . TFCS
. . dlconnectedTrCHList
. . . CphyTrchConfigReq_setseq_1
. . . . (IntegerType)trchid = 10
. . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 148
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional = 1
. . . . . . (IntegerType)rateMatchingAttribute = 192
. . . . . . (CRC_Size)crc_Size = 3
. . TFCS
. . . ExplicitTFCS_Configuration
. . . . TFCS_ReconfAdd
. . . . . ctfcSize
. . . . . . ctfc2Bit
. . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . (IntegerType)ctfc2 = 0
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . (IntegerType)ctfc2 = 1
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . fdd
. . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 11
. . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
- Constraint:
ca_DCH_148_TTI_10_DL_Info
- BinaryMessage:
30 5b 02 01 00 02 01 1a 0a 01 00 30 50 02 02 00 88 30 26 30 24 02 01 0a 0a 01 00 30 1c 30 0e 30 0c 02 02 00 94 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 c0 0a 01 03 30 22 30 30 1f 30 08 02 01 00 30 03 02 01 00 30 13 02 01 01 30 0e 30 0c 30 30 03 02 01 0b 02 01 0f 02 01 00

- No.: 2506
- Timestamp: 10:52:37:519_0
- RFN: 3745
- Chip: 12032
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Config_CNF
- Source: ts_SS_1DCH_DCCH_Modify LINE 7
- Message Structure:
CPHY_TrCH_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
ca_TrChCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 1a

- No.: 2507
- Timestamp: 10:52:37:562_0
- RFN: 3749
- Chip: 20992
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_SS_1DCH_DCCH_Modify LINE 8
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
. (RatType)ratType = 0
. configMessage
. . CmacConfigReq
. . . SS_ActivationTime
. . . . (IntegerType)activationCFN = 136
. . . UE_Info
. . . . U_RNTI
. . . . (BitStringType)c_RNTI[16] = -
. . . TrCHInfo
. . . . ulconnectedTrCHList
. . . . TFCS
. . . . dlconnectedTrCHList
. . . . . TrCHInfo_setseq_1
. . . . . . (IntegerType)trchid = 10
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 148
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . (IntegerType)rateMatchingAttribute = 192
. . . . . . . . (CRC_Size)crc_Size = 3
. . . . TFCS
. . . . . ExplicitTFCS_Configuration
. . . . . . TFCS_ReconfAdd
. . . . . . . ctfcSize
. . . . . . . . ctfc2Bit
. . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . (IntegerType)ctfc2 = 0
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . (IntegerType)ctfc2 = 1
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 11
. . . . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . TrCH_LogCHMappingList1
. . . . ulconnectedTrCHList
. . . . dlconnectedTrCHList
. . . . . TrCH_LogCHMappingList1_setseq_1
. . . . . . (IntegerType)trchid = 10
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 1
. . . . . . . . (IntegerType)rB_Identity = 1
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 2
. . . . . . . . (IntegerType)rB_Identity = 2
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 3
. . . . . . . . (IntegerType)rB_Identity = 3
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 4
. . . . . . . . (IntegerType)rB_Identity = 4
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_CMAC_ReconfigInfo
- BinaryMessage:
30 81 c8 02 01 ff 02 01 1a 0a 01 00 30 81 bc 02 02 00 88 30 00 30 49 30 23 30 21 02 01 0a 30 1c 30 0e 30 0c 02 02 00 94 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 c0 0a 01 03 30 22 30 30 1f 30 08 02 01 00 30 03 02 01 00 30 13 02 01 01 30 0e 30 0c 30 30 03 02 01 0b 02 01 0f 02 01 00 30 69 30 67 30 65 02 01 0a 30 60 30 16 30 11 0a 01 00 0a 01 00 02 01 01 0a 01 04 05 00 02 01 01 02 01 01 30 16 30 11 0a 01 00 0a 01 00 02 01 02 0a 01 04 05 00 02 01 02 02 01 02 30 16 30 11 0a 01 00 0a 01 00 02 01 03 0a 01 04 05 00 02 01 03 02 01 03 30 16 30 11 0a 01 00 0a 01 00 02 01 04 0a 01 04 05 00 02 01 04 02 01 04

- No.: 2508
- Timestamp: 10:52:37:571_0
- RFN: 3750
- Chip: 17152
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_SS_1DCH_DCCH_Modify LINE 9
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 1a

- No.: 2509
- Timestamp: 10:52:37:577_0
- RFN: 3751
- Chip: 2048
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Modify_REQ
- Source: ts_SS_1DCH_DCCH_Modify LINE 10
- Message Structure:
CPHY_RL_Modify_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
. (RatType)ratType = 0
. CphyRlModifyReq
. . SS_ActivationTime
. . . (IntegerType)activationCFN = 136
. . physicalChannelInfo
. . . DPCHInfo
. . . . UL_DPCH_Info
. . . . . UL_DPCH_PowerControlInfo
. . . . . . fdd
. . . . . . . (IntegerType)dpcch_PowerOffset = -40
. . . . . . . (IntegerType)pc_Preamble = 1
. . . . . . . (IntegerType)sRB_delay = 7
. . . . . . . PowerControlAlgorithm
. . . . . . . . (IntegerType)algorithm1 = 1
. . . . . modeSpecificInfo
. . . . . . fdd
. . . . . . . (ScramblingCodeType)scramblingCodeType = 1
. . . . . . . (IntegerType)scramblingCode = 0
. . . . . . . (IntegerType)numberOfDPDCH = -
. . . . . . . (SpreadingFactor)spreadingFactor = 4
. . . . . . . (BooleanType)tfci_Existence = TRUE
. . . . . . . (IntegerType)numberOfFBI_Bits = -
. . . . . . . (PuncturingLimit)puncturingLimit = 15
. . . . DL_DPCHInfo
- Constraint:
ca_UL_DPCH_ModifyInfo
- BinaryMessage:
30 34 02 01 00 02 01 14 0a 01 00 30 29 02 02 00 88 30 23 30 21 30 30 0c 02 01 d8 02 01 01 02 01 07 02 01 01 30 30 0f 0a 01 01 02 01 00 0a 01 04 01 01 ff 0a 01 0f

- No.: 2513
- Timestamp: 10:52:37:586_0
- RFN: 3752
- Chip: 1280
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Modify_CNF
- Source: ts_SS_1DCH_DCCH_Modify LINE 11
- Message Structure:
CPHY_RL_Modify_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_RL_ModifyCnf
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 2514
- Timestamp: 10:52:37:596_0
- RFN: 3752
- Chip: 36864
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Config_REQ
- Source: ts_SS_1DCH_DCCH_Modify LINE 12
- Message Structure:
CPHY_TrCH_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
. (RatType)ratType = 0
. CphyTrchConfigReq
. . SS_ActivationTime
. . . (IntegerType)activationCFN = 136
. . ulconnectedTrCHList
. . . CphyTrchConfigReq_setseq_0
. . . . (IntegerType)trchid = 5
. . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 148
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional = 1
. . . . . . (IntegerType)rateMatchingAttribute = 192
. . . . . . (CRC_Size)crc_Size = 3
. . TFCS
. . . ExplicitTFCS_Configuration
. . . . TFCS_ReconfAdd
. . . . . ctfcSize
. . . . . . ctfc2Bit
. . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . (IntegerType)ctfc2 = 0
. . . . . . . . PowerOffsetInformation
. . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . (IntegerType)ctfc2 = 1
. . . . . . . . PowerOffsetInformation
. . dlconnectedTrCHList
. . TFCS
- Constraint:
ca_DCH_148_TTI_10_UL_Info
- BinaryMessage:
30 46 02 01 00 02 01 14 0a 01 00 30 3b 02 02 00 88 30 26 30 24 02 01 05 0a 01 00 30 1c 30 0e 30 0c 02 02 00 94 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 c0 0a 01 03 30 0d 30 30 0a 30 03 02 01 00 30 03 02 01 01

- No.: 2518
- Timestamp: 10:52:37:609_0
- RFN: 3754
- Chip: 10752
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Config_CNF
- Source: ts_SS_1DCH_DCCH_Modify LINE 13
- Message Structure:
CPHY_TrCH_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_TrChCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 2519
- Timestamp: 10:52:37:646_0
- RFN: 3757
- Chip: 37376
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_SS_1DCH_DCCH_Modify LINE 14
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
. (RatType)ratType = 0
. configMessage
. . CmacConfigReq
. . . SS_ActivationTime
. . . . (IntegerType)activationCFN = 136
. . . UE_Info
. . . . U_RNTI
. . . . (BitStringType)c_RNTI[16] = -
. . . TrCHInfo
. . . . ulconnectedTrCHList
. . . . . TrCHInfo_setseq_0
. . . . . . (IntegerType)trchid = 5
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 148
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . (IntegerType)rateMatchingAttribute = 192
. . . . . . . . (CRC_Size)crc_Size = 3
. . . . TFCS
. . . . . ExplicitTFCS_Configuration
. . . . . . TFCS_ReconfAdd
. . . . . . . ctfcSize
. . . . . . . . ctfc2Bit
. . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . (IntegerType)ctfc2 = 0
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . (IntegerType)ctfc2 = 1
. . . . . . . . . . PowerOffsetInformation
. . . . dlconnectedTrCHList
. . . . TFCS
. . . TrCH_LogCHMappingList1
. . . . ulconnectedTrCHList
. . . . . TrCH_LogCHMappingList1_setseq_0
. . . . . . (IntegerType)trchid = 5
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . (IntegerType)rB_Identity = 1
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . (IntegerType)rB_Identity = 2
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . (IntegerType)rB_Identity = 3
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . (IntegerType)rB_Identity = 4
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . dlconnectedTrCHList
- Constraint:
ca_CMAC_ReconfigInfo
- BinaryMessage:
30 81 9f 02 01 ff 02 01 14 0a 01 00 30 81 93 02 02 00 88 30 00 30 34 30 23 30 21 02 01 05 30 1c 30 0e 30 0c 02 02 00 94 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 c0 0a 01 03 30 0d 30 30 0a 30 03 02 01 00 30 03 02 01 01 30 55 30 53 30 51 02 01 05 30 4c 30 11 30 0c 0a 01 00 0a 01 00 02 01 01 0a 01 04 02 01 01 30 11 30 0c 0a 01 00 0a 01 00 02 01 02 0a 01 04 02 01 02 30 11 30 0c 0a 01 00 0a 01 00 02 01 03 0a 01 04 02 01 03 30 11 30 0c 0a 01 00 0a 01 00 02 01 04 0a 01 04 02 01 04

- No.: 2523
- Timestamp: 10:52:37:655_0
- RFN: 3758
- Chip: 34048
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_SS_1DCH_DCCH_Modify LINE 15
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 14

- No.: 2533
- Timestamp: 10:52:37:658_0
- RFN: 3759
- Chip: 6656
- Event: Start Timer
- Source: ts_RRC_ReceiveRB_RelCmpl LINE 2
- Message Structure:
no details available
- Constraint:
t_WaitMS (13500 Ms)
- BinaryMessage:

- No.: 2537
- Timestamp: 10:52:39:899_0
- RFN: 3983
- Chip: 12288
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_IND
- Source: ts_RRC_ReceiveRB_RelCmpl LINE 3
- Message Structure:
RLC_AM_DATA_IND
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. IntegrityResult
. . (IntegrityStatus)integrityUsed = 0
. aM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "11100111101110000111111101010101"
. . . . (IntegerType)rrc_MessageSequenceNumber = 3
. . . UL_DCCH_MessageType
. . . . RadioBearerReleaseComplete
. . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . IntegrityProtActivationInfo
. . . . . (IntegerType)ul_TimingAdvance = 0
. . . . . (IntegerType)count_C_ActivationTime = 0
. . . . . UL_CounterSynchronisationInfo
. . . . . laterNonCriticalExtensions
. . . . . . (BitStringType)radioBearerReleaseComplete_r3_add_ext = 0
. . . . . . nonCriticalExtensions
- Constraint:
car_RB_RelCmpl
- BinaryMessage:
30 10 02 01 ff 02 01 02 0a 01 00 f3 dc 3f aa 9b 40 00

- No.: 2538
- Timestamp: 10:52:39:900_0
- RFN: 3983
- Chip: 16896
- Event: Cancel Timer
- Source: ts_RRC_ReceiveRB_RelCmpl LINE 3
- Message Structure:
no details available
- Constraint:
t_WaitMS
- BinaryMessage:

- No.: 2539
- Timestamp: 10:52:39:900_1
- RFN: 3983
- Chip: 17664
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ReceiveRB_RelCmpl LINE 3
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2568
- Timestamp: 10:52:39:929_0
- RFN: 3986
- Chip: 14336
- Event: Send
- PCO: CPHY
- Message: CPHY_Frame_Number_REQ
- Source: ts_RRC_SetUpRAB_AM_7_RLC LINE 2
- Message Structure:
CPHY_Frame_Number_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
cas_GetFrameNum
- BinaryMessage:
30 06 02 01 00 02 01 1a

- No.: 2572
- Timestamp: 10:52:39:938_0
- RFN: 3987
- Chip: 9216
- Event: Receive
- PCO: CPHY
- Message: CPHY_Frame_Number_CNF
- Source: ts_RRC_SetUpRAB_AM_7_RLC LINE 3
- Message Structure:
CPHY_Frame_Number_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
. (IntegerType)frameNumber = 146
- Constraint:
car_GetFrameNum
- BinaryMessage:
30 0a 02 01 00 02 01 1a 02 02 00 92

- No.: 2576
- Timestamp: 10:52:39:983_0
- RFN: 3991
- Chip: 28416
- Event: Send
- PCO: AM
- Message: RLC_AM_DATA_REQ
- Source: ts_RRC_SetUpRAB_AM_7_RLC:lt_SendRAB_SetupCS_OrPS LINE 4
- Message Structure:
RLC_AM_DATA_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. AmConfirmationRequest
. . (IntegerType)confirmationRequested = 0
. aM_message
. . DL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00000000000000000000000000000000"
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . DL_DCCH_MessageType
. . . . RadioBearerSetup
. . . . . r3
. . . . . . RadioBearerSetup_r3_IEs
. . . . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . . . IntegrityProtectionModeInfo
. . . . . . . CipheringModeInfo
. . . . . . . (IntegerType)activationTime = 136
. . . . . . . U_RNTI
. . . . . . . (BitStringType)new_C_RNTI[16] = -
. . . . . . . (RRC_StateIndicator)rrc_StateIndicator = 0
. . . . . . . (IntegerType)utran_DRX_CycleLengthCoeff = -
. . . . . . . (BitStringType)ura_Identity[0] = -
. . . . . . . CN_InformationInfo
. . . . . . . SRB_InformationSetupList
. . . . . . . RAB_InformationSetupList
. . . . . . . . RAB_InformationSetup
. . . . . . . . . RAB_Info
. . . . . . . . . . RAB_Identity
. . . . . . . . . . . (BitStringType)gsm_MAP_RAB_Identity[8] = '00000101'B
. . . . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = 1
. . . . . . . . . . (BitStringType)nas_Synchronisation_Indicator[0] = -
. . . . . . . . . . (Re_EstablishmentTimer)re_EstablishmentTimer = 0
. . . . . . . . . RB_InformationSetupList
. . . . . . . . . . RB_InformationSetup
. . . . . . . . . . . (IntegerType)rb_Identity = 20
. . . . . . . . . . . PDCP_Info
. . . . . . . . . . . RLC_InfoChoice
. . . . . . . . . . . . RLC_Info
. . . . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . . . MaxDAT_Retransmissions
. . . . . . . . . . . . . . . . . (MaxDAT)maxDAT = 3
. . . . . . . . . . . . . . . . . (TimerMRW)timerMRW = 13
. . . . . . . . . . . . . . . . . (MaxMRW)maxMRW = 1
. . . . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize = 5
. . . . . . . . . . . . . . . (TimerRST)timerRST = 9
. . . . . . . . . . . . . . . (MaxRST)max_RST = 1
. . . . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit = -
. . . . . . . . . . . . . . . . (TimerPoll)timerPoll = -
. . . . . . . . . . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . . . . . . . . . (Poll_SDU)poll_SDU = -
. . . . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = FALSE
. . . . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = FALSE
. . . . . . . . . . . . . . . . (PollWindow)pollWindow = -
. . . . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic = 7
. . . . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize = 5
. . . . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit = -
. . . . . . . . . . . . . . . . (TimerEPC)timerEPC = -
. . . . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . . . . . . . . RB_MappingInfo
. . . . . . . . . . . . RB_MappingOption
. . . . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . . . (IntegerType)dch = 1
. . . . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 7
. . . . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 7
. . . . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . . . (IntegerType)dch = 6
. . . . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 7
. . . . . . . RB_InformationAffectedList
. . . . . . . DL_CounterSynchronisationInfo
. . . . . . . UL_CommonTransChInfo
. . . . . . . . TFC_Subset
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . TFCS
. . . . . . . . . . . ExplicitTFCS_Configuration
. . . . . . . . . . . . TFCS_ReconfAdd
. . . . . . . . . . . . . ctfcSize
. . . . . . . . . . . . . . ctfc4Bit
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . . . . . . . (IntegerType)ctfc4 = 0
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . . . . . . . (IntegerType)ctfc4 = 1
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . . . . . . . (IntegerType)ctfc4 = 2
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . . . . . . . (IntegerType)ctfc4 = 3
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 11
. . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . UL_DeletedTransChInfoList
. . . . . . . UL_AddReconfTransChInfoList
. . . . . . . . UL_AddReconfTransChInformation
. . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType = 0
. . . . . . . . . (IntegerType)transportChannelIdentity = 1
. . . . . . . . . TransportFormatSet
. . . . . . . . . . DedicatedTransChTFS
. . . . . . . . . . . tti
. . . . . . . . . . . . DedicatedDynamicTF_InfoList
. . . . . . . . . . . . . DedicatedDynamicTF_Info
. . . . . . . . . . . . . . rlc_Size
. . . . . . . . . . . . . . . OctetModeRLC_SizeInfoType1
. . . . . . . . . . . . . . . . (IntegerType)sizeType1 = 16
. . . . . . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . LogicalChannelList
. . . . . . . . . . . SemistaticTF_Information
. . . . . . . . . . . . ChannelCodingType
. . . . . . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . . . . . (IntegerType)rateMatchingAttribute = 155
. . . . . . . . . . . . (CRC_Size)crc_Size = 3
. . . . . . . . UL_AddReconfTransChInformation
. . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType = 0
. . . . . . . . . (IntegerType)transportChannelIdentity = 5
. . . . . . . . . TransportFormatSet
. . . . . . . . . . DedicatedTransChTFS
. . . . . . . . . . . tti
. . . . . . . . . . . . DedicatedDynamicTF_InfoList
. . . . . . . . . . . . . DedicatedDynamicTF_Info
. . . . . . . . . . . . . . rlc_Size
. . . . . . . . . . . . . . . BitModeRLC_SizeInfo
. . . . . . . . . . . . . . . . sizeType2
. . . . . . . . . . . . . . . . . (IntegerType)part1 = 2
. . . . . . . . . . . . . . . . . (IntegerType)part2 = -
. . . . . . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . LogicalChannelList
. . . . . . . . . . . SemistaticTF_Information
. . . . . . . . . . . . ChannelCodingType
. . . . . . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . . . . . (IntegerType)rateMatchingAttribute = 170
. . . . . . . . . . . . (CRC_Size)crc_Size = 3
. . . . . . . modeSpecificTransChInfo
. . . . . . . . fdd
. . . . . . . . . (IntegerType)cpch_SetID = -
. . . . . . . . . DRAC_StaticInformationList
. . . . . . . DL_CommonTransChInfo
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . dl_Parameters
. . . . . . . DL_DeletedTransChInfoList
. . . . . . . DL_AddReconfTransChInfoList
. . . . . . . . DL_AddReconfTransChInformation
. . . . . . . . . (DL_TrCH_Type)dl_TransportChannelType = 0
. . . . . . . . . (IntegerType)dl_transportChannelIdentity = 6
. . . . . . . . . tfs_SignallingMode
. . . . . . . . . . UL_TransportChannelIdentity
. . . . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType = 0
. . . . . . . . . . . (IntegerType)ul_TransportChannelIdentity = 1
. . . . . . . . . QualityTarget
. . . . . . . . . . (IntegerType)bler_QualityValue = -20
. . . . . . . . . TM_SignallingInfo
. . . . . . . . DL_AddReconfTransChInformation
. . . . . . . . . (DL_TrCH_Type)dl_TransportChannelType = 0
. . . . . . . . . (IntegerType)dl_transportChannelIdentity = 10
. . . . . . . . . tfs_SignallingMode
. . . . . . . . . . UL_TransportChannelIdentity
. . . . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType = 0
. . . . . . . . . . . (IntegerType)ul_TransportChannelIdentity = 5
. . . . . . . . . QualityTarget
. . . . . . . . . . (IntegerType)bler_QualityValue = -20
. . . . . . . . . TM_SignallingInfo
. . . . . . . FrequencyInfo
. . . . . . . (IntegerType)maxAllowedUL_TX_Power = 33
. . . . . . . UL_ChannelRequirement
. . . . . . . . UL_DPCH_Info
. . . . . . . . . UL_DPCH_PowerControlInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (IntegerType)dpcch_PowerOffset = -40
. . . . . . . . . . . (IntegerType)pc_Preamble = 1
. . . . . . . . . . . (IntegerType)sRB_delay = 7
. . . . . . . . . . . PowerControlAlgorithm
. . . . . . . . . . . . (IntegerType)algorithm1 = 1
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (ScramblingCodeType)scramblingCodeType = 1
. . . . . . . . . . . (IntegerType)scramblingCode = 0
. . . . . . . . . . . (IntegerType)numberOfDPDCH = -
. . . . . . . . . . . (SpreadingFactor)spreadingFactor = 4
. . . . . . . . . . . (BooleanType)tfci_Existence = TRUE
. . . . . . . . . . . (IntegerType)numberOfFBI_Bits = -
. . . . . . . . . . . (PuncturingLimit)puncturingLimit = 15
. . . . . . . modeSpecificPhysChInfo
. . . . . . . . fdd
. . . . . . . . . DL_PDSCH_Information
. . . . . . . DL_CommonInformation
. . . . . . . . DL_DPCH_InfoCommon
. . . . . . . . . cfnHandling
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . DL_DPCH_PowerControlInfo
. . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . (DPC_Mode)dpc_Mode = 0
. . . . . . . . . . . (IntegerType)powerOffsetPilot_pdpdch = 0
. . . . . . . . . . . Dl_rate_matching_restriction
. . . . . . . . . . . SF512_AndPilot
. . . . . . . . . . . . (PilotBits128)sfd128 = 0
. . . . . . . . . . . (PositionFixedOrFlexible)positionFixedOrFlexible = 1
. . . . . . . . . . . (BooleanType)tfci_Existence = TRUE
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . (IntegerType)defaultDPCH_OffsetValue = -
. . . . . . . . . . DPCH_CompressedModeInfo
. . . . . . . . . . (TX_DiversityMode)tx_DiversityMode = 0
. . . . . . . . . . SSDT_Information
. . . . . . . DL_InformationPerRL_List
. . . . . . . . DL_InformationPerRL
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . PrimaryCPICH_Info
. . . . . . . . . . . . (IntegerType)primaryScramblingCode = 100
. . . . . . . . . . . PDSCH_SHO_DCH_Info
. . . . . . . . . . . PDSCH_CodeMapping
. . . . . . . . . DL_DPCH_InfoPerRL
. . . . . . . . . . fdd
. . . . . . . . . . . (PCPICH_UsageForChannelEst)pCPICH_UsageForChannelEst = 0
. . . . . . . . . . . (IntegerType)dpch_FrameOffset = 0
. . . . . . . . . . . SecondaryCPICH_Info
. . . . . . . . . . . DL_ChannelisationCodeList
. . . . . . . . . . . . DL_ChannelisationCode
. . . . . . . . . . . . . (IntegerType)secondaryScramblingCode = 1
. . . . . . . . . . . . . SF512_AndCodeNumber
. . . . . . . . . . . . . . (IntegerType)sf128 = 0
. . . . . . . . . . . . . (ScramblingCodeChange)scramblingCodeChange = -
. . . . . . . . . . . (IntegerType)tpc_CombinationIndex = 0
. . . . . . . . . . . (SSDT_CellIdentity)ssdt_CellIdentity = -
. . . . . . . . . . . (ClosedLoopTimingAdjMode)closedLoopTimingAdjMode = -
. . . . . . . . . SCCPCH_InfoForFACH
. . . . . . v3a0NonCriticalExtensions
. . . . . . . RadioBearerSetup_v3a0ext
. . . . . . . . (BitStringType)new_DSCH_RNTI[16] = -
. . . . . . . laterNonCriticalExtensions
- Constraint:
cas_RB_SetUpAM_WithCnf
- BinaryMessage:
30 4f 02 01 ff 02 01 02 02 01 00 80 00 00 00 03 92 04 ba f2 20 00 16 09 b3 1e 95 92 09 ca 88 d0 0c e4 2b 10 20 1c 12 29 24 99 5f 81 00 41 20 11 1c d3 10 80 44 11 1d 4b 06 18 58 15 c4 c4 ae 9a 54 7a 20 00 00 13 e4 80 56 20 40 c8 00 01 05 00 00

- No.: 2581
- Timestamp: 10:52:40:138_0
- RFN: 4007
- Chip: 8704
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_CNF
- Source: ts_RRC_SetUpRAB_AM_7_RLC LINE 6
- Message Structure:
RLC_AM_DATA_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. (IntegerType)mui = 0
- Constraint:
car_AM_DataMuiCnf
- BinaryMessage:
30 09 02 01 ff 02 01 02 02 01 00

- No.: 2588
- Timestamp: 10:52:40:273_0
- RFN: 4020
- Chip: 28416
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Modify_REQ
- Source: ts_SS_2DCH_Modify LINE 3
- Message Structure:
CPHY_RL_Modify_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
. (RatType)ratType = 0
. CphyRlModifyReq
. . SS_ActivationTime
. . . (IntegerType)activationCFN = 136
. . physicalChannelInfo
. . . DPCHInfo
. . . . UL_DPCH_Info
. . . . DL_DPCHInfo
. . . . . DL_CommonInformation
. . . . . . DL_DPCH_InfoCommon
. . . . . . . cfnHandling
. . . . . . . modeSpecificInfo
. . . . . . . . fdd
. . . . . . . . . DL_DPCH_PowerControlInfo
. . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . fdd
. . . . . . . . . . . . (DPC_Mode)dpc_Mode = 0
. . . . . . . . . (IntegerType)powerOffsetPilot_pdpdch = 0
. . . . . . . . . Dl_rate_matching_restriction
. . . . . . . . . SF512_AndPilot
. . . . . . . . . . (PilotBits128)sfd128 = 0
. . . . . . . . . (PositionFixedOrFlexible)positionFixedOrFlexible = 1
. . . . . . . . . (BooleanType)tfci_Existence = TRUE
. . . . . . modeSpecificInfo
. . . . . . . fdd
. . . . . . . . (IntegerType)defaultDPCH_OffsetValue = -
. . . . . . . . DPCH_CompressedModeInfo
. . . . . . . . (TX_DiversityMode)tx_DiversityMode = 0
. . . . . . . . SSDT_Information
. . . . . DL_DPCH_InfoPerRL
. . . . . . fdd
. . . . . . . (PCPICH_UsageForChannelEst)pCPICH_UsageForChannelEst = 0
. . . . . . . (IntegerType)dpch_FrameOffset = 0
. . . . . . . SecondaryCPICH_Info
. . . . . . . DL_ChannelisationCodeList
. . . . . . . . DL_ChannelisationCode
. . . . . . . . . (IntegerType)secondaryScramblingCode = 1
. . . . . . . . . SF512_AndCodeNumber
. . . . . . . . . . (IntegerType)sf128 = 0
. . . . . . . . . (ScramblingCodeChange)scramblingCodeChange = -
. . . . . . . (IntegerType)tpc_CombinationIndex = 0
. . . . . . . (SSDT_CellIdentity)ssdt_CellIdentity = -
. . . . . . . (ClosedLoopTimingAdjMode)closedLoopTimingAdjMode = -
. . . . . (IntegerType)powerOffsetOfTFCI_PO1 = 0
. . . . . (IntegerType)powerOffsetOfTPC_PO2 = 0
. . . . . (IntegerType)powerOffsetOfPILOT_PO3 = 0
. . . . . (IntegerType)dl_TxPower = -5
. . . . . (IntegerType)dl_TxPowerMax = 15
. . . . . (IntegerType)dl_TxPowerMin = -35
- Constraint:
ca_DL_DPCH_ModifyInfo
- BinaryMessage:
30 5e 02 01 00 02 01 1a 0a 01 00 30 53 02 02 00 88 30 4d 30 4b 30 21 30 19 05 00 30 30 14 30 06 30 30 03 0a 01 00 02 01 00 0a 01 00 0a 01 01 01 01 ff 30 30 03 0a 01 00 30 30 13 0a 01 00 02 01 00 30 08 30 06 02 01 01 02 01 00 02 01 00 02 01 00 02 01 00 02 01 00 02 01 fb 02 01 0f 02 01 dd

- No.: 2592
- Timestamp: 10:52:40:321_0
- RFN: 4025
- Chip: 20736
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Modify_CNF
- Source: ts_SS_2DCH_Modify LINE 4
- Message Structure:
CPHY_RL_Modify_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
ca_RL_ModifyCnf
- BinaryMessage:
30 06 02 01 00 02 01 1a

- No.: 2593
- Timestamp: 10:52:40:349_0
- RFN: 4028
- Chip: 9472
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Config_REQ
- Source: ts_SS_2DCH_Modify LINE 5
- Message Structure:
CPHY_TrCH_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
. (RatType)ratType = 0
. CphyTrchConfigReq
. . SS_ActivationTime
. . . (IntegerType)activationCFN = 136
. . ulconnectedTrCHList
. . TFCS
. . dlconnectedTrCHList
. . . CphyTrchConfigReq_setseq_1
. . . . (IntegerType)trchid = 6
. . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 144
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional = 1
. . . . . . (IntegerType)rateMatchingAttribute = 155
. . . . . . (CRC_Size)crc_Size = 3
. . . CphyTrchConfigReq_setseq_1
. . . . (IntegerType)trchid = 10
. . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 148
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional = 1
. . . . . . (IntegerType)rateMatchingAttribute = 170
. . . . . . (CRC_Size)crc_Size = 3
. . TFCS
. . . ExplicitTFCS_Configuration
. . . . TFCS_ReconfAdd
. . . . . ctfcSize
. . . . . . ctfc4Bit
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 0
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 1
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 2
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 3
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . fdd
. . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 9
. . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
- Constraint:
ca_TrChCfgInfo
- BinaryMessage:
30 81 96 02 01 00 02 01 1a 0a 01 00 30 81 8a 02 02 00 88 30 4c 30 24 02 01 06 0a 01 00 30 1c 30 0e 30 0c 02 02 00 90 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 9b 0a 01 03 30 24 02 01 0a 0a 01 00 30 1c 30 0e 30 0c 02 02 00 94 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 aa 0a 01 03 30 36 30 30 33 30 08 02 01 00 30 03 02 01 00 30 08 02 01 01 30 03 02 01 00 30 08 02 01 02 30 03 02 01 00 30 13 02 01 03 30 0e 30 0c 30 30 03 02 01 09 02 01 0f 02 01 00

- No.: 2597
- Timestamp: 10:52:40:403_0
- RFN: 4033
- Chip: 26880
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Config_CNF
- Source: ts_SS_2DCH_Modify LINE 6
- Message Structure:
CPHY_TrCH_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
ca_TrChCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 1a

- No.: 2598
- Timestamp: 10:52:40:464_0
- RFN: 4039
- Chip: 31744
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_SS_2DCH_Modify LINE 7
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
. (RatType)ratType = 0
. configMessage
. . CmacConfigReq
. . . SS_ActivationTime
. . . . (IntegerType)activationCFN = 136
. . . UE_Info
. . . . U_RNTI
. . . . (BitStringType)c_RNTI[16] = -
. . . TrCHInfo
. . . . ulconnectedTrCHList
. . . . TFCS
. . . . dlconnectedTrCHList
. . . . . TrCHInfo_setseq_1
. . . . . . (IntegerType)trchid = 6
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 144
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . (IntegerType)rateMatchingAttribute = 155
. . . . . . . . (CRC_Size)crc_Size = 3
. . . . . TrCHInfo_setseq_1
. . . . . . (IntegerType)trchid = 10
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 148
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . (IntegerType)rateMatchingAttribute = 170
. . . . . . . . (CRC_Size)crc_Size = 3
. . . . TFCS
. . . . . ExplicitTFCS_Configuration
. . . . . . TFCS_ReconfAdd
. . . . . . . ctfcSize
. . . . . . . . ctfc4Bit
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 0
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 1
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 2
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 3
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 9
. . . . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . TrCH_LogCHMappingList1
. . . . ulconnectedTrCHList
. . . . dlconnectedTrCHList
. . . . . TrCH_LogCHMappingList1_setseq_1
. . . . . . (IntegerType)trchid = 6
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 7
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 5
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 7
. . . . . . . . (IntegerType)rB_Identity = -12
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . TrCH_LogCHMappingList1_setseq_1
. . . . . . (IntegerType)trchid = 10
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 1
. . . . . . . . (IntegerType)rB_Identity = 1
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 2
. . . . . . . . (IntegerType)rB_Identity = 2
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 3
. . . . . . . . (IntegerType)rB_Identity = 3
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 4
. . . . . . . . (IntegerType)rB_Identity = 4
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_CMAC_ReconfigInfo
- BinaryMessage:
30 82 01 22 02 01 ff 02 01 1a 0a 01 00 30 82 01 15 02 02 00 88 30 00 30 81 80 30 46 30 21 02 01 06 30 1c 30 0e 30 0c 02 02 00 90 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 9b 0a 01 03 30 21 02 01 0a 30 1c 30 0e 30 0c 02 02 00 94 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 aa 0a 01 03 30 36 30 30 33 30 08 02 01 00 30 03 02 01 00 30 08 02 01 01 30 03 02 01 00 30 08 02 01 02 30 03 02 01 00 30 13 02 01 03 30 0e 30 0c 30 30 03 02 01 09 02 01 0f 02 01 00 30 81 89 30 81 86 30 1d 02 01 06 30 18 30 16 30 11 0a 01 00 0a 01 00 02 01 07 0a 01 05 05 00 02 01 07 02 01 f4 30 65 02 01 0a 30 60 30 16 30 11 0a 01 00 0a 01 00 02 01 01 0a 01 04 05 00 02 01 01 02 01 01 30 16 30 11 0a 01 00 0a 01 00 02 01 02 0a 01 04 05 00 02 01 02 02 01 02 30 16 30 11 0a 01 00 0a 01 00 02 01 03 0a 01 04 05 00 02 01 03 02 01 03 30 16 30 11 0a 01 00 0a 01 00 02 01 04 0a 01 04 05 00 02 01 04 02 01 04

- No.: 2599
- Timestamp: 10:52:40:500_0
- RFN: 4043
- Chip: 15872
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_SS_2DCH_Modify LINE 8
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 1a

- No.: 2600
- Timestamp: 10:52:40:529_0
- RFN: 4046
- Chip: 13056
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Modify_REQ
- Source: ts_SS_2DCH_Modify LINE 9
- Message Structure:
CPHY_RL_Modify_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
. (RatType)ratType = 0
. CphyRlModifyReq
. . SS_ActivationTime
. . . (IntegerType)activationCFN = 136
. . physicalChannelInfo
. . . DPCHInfo
. . . . UL_DPCH_Info
. . . . . UL_DPCH_PowerControlInfo
. . . . . . fdd
. . . . . . . (IntegerType)dpcch_PowerOffset = -40
. . . . . . . (IntegerType)pc_Preamble = 1
. . . . . . . (IntegerType)sRB_delay = 7
. . . . . . . PowerControlAlgorithm
. . . . . . . . (IntegerType)algorithm1 = 1
. . . . . modeSpecificInfo
. . . . . . fdd
. . . . . . . (ScramblingCodeType)scramblingCodeType = 1
. . . . . . . (IntegerType)scramblingCode = 0
. . . . . . . (IntegerType)numberOfDPDCH = -
. . . . . . . (SpreadingFactor)spreadingFactor = 4
. . . . . . . (BooleanType)tfci_Existence = TRUE
. . . . . . . (IntegerType)numberOfFBI_Bits = -
. . . . . . . (PuncturingLimit)puncturingLimit = 15
. . . . DL_DPCHInfo
- Constraint:
ca_UL_DPCH_ModifyInfo
- BinaryMessage:
30 34 02 01 00 02 01 14 0a 01 00 30 29 02 02 00 88 30 23 30 21 30 30 0c 02 01 d8 02 01 01 02 01 07 02 01 01 30 30 0f 0a 01 01 02 01 00 0a 01 04 01 01 ff 0a 01 0f

- No.: 2604
- Timestamp: 10:52:40:580_0
- RFN: 4051
- Chip: 16128
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Modify_CNF
- Source: ts_SS_2DCH_Modify LINE 10
- Message Structure:
CPHY_RL_Modify_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_RL_ModifyCnf
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 2605
- Timestamp: 10:52:40:610_0
- RFN: 4054
- Chip: 16128
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Config_REQ
- Source: ts_SS_2DCH_Modify LINE 11
- Message Structure:
CPHY_TrCH_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
. (RatType)ratType = 0
. CphyTrchConfigReq
. . SS_ActivationTime
. . . (IntegerType)activationCFN = 136
. . ulconnectedTrCHList
. . . CphyTrchConfigReq_setseq_0
. . . . (IntegerType)trchid = 1
. . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 144
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional = 1
. . . . . . (IntegerType)rateMatchingAttribute = 155
. . . . . . (CRC_Size)crc_Size = 3
. . . CphyTrchConfigReq_setseq_0
. . . . (IntegerType)trchid = 5
. . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 148
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional = 1
. . . . . . (IntegerType)rateMatchingAttribute = 170
. . . . . . (CRC_Size)crc_Size = 3
. . TFCS
. . . ExplicitTFCS_Configuration
. . . . TFCS_ReconfAdd
. . . . . ctfcSize
. . . . . . ctfc4Bit
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 0
. . . . . . . . PowerOffsetInformation
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 1
. . . . . . . . PowerOffsetInformation
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 2
. . . . . . . . PowerOffsetInformation
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 3
. . . . . . . . PowerOffsetInformation
. . dlconnectedTrCHList
. . TFCS
- Constraint:
ca_TrChCfgInfo
- BinaryMessage:
30 76 02 01 00 02 01 14 0a 01 00 30 6b 02 02 00 88 30 4c 30 24 02 01 01 0a 01 00 30 1c 30 0e 30 0c 02 02 00 90 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 9b 0a 01 03 30 24 02 01 05 0a 01 00 30 1c 30 0e 30 0c 02 02 00 94 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 aa 0a 01 03 30 17 30 30 14 30 03 02 01 00 30 03 02 01 01 30 03 02 01 02 30 03 02 01 03

- No.: 2609
- Timestamp: 10:52:40:662_0
- RFN: 4059
- Chip: 20992
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Config_CNF
- Source: ts_SS_2DCH_Modify LINE 12
- Message Structure:
CPHY_TrCH_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_TrChCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 2610
- Timestamp: 10:52:40:736_0
- RFN: 4067
- Chip: 512
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_SS_2DCH_Modify LINE 13
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
. (RatType)ratType = 0
. configMessage
. . CmacConfigReq
. . . SS_ActivationTime
. . . . (IntegerType)activationCFN = 136
. . . UE_Info
. . . . U_RNTI
. . . . (BitStringType)c_RNTI[16] = -
. . . TrCHInfo
. . . . ulconnectedTrCHList
. . . . . TrCHInfo_setseq_0
. . . . . . (IntegerType)trchid = 1
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 144
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . (IntegerType)rateMatchingAttribute = 155
. . . . . . . . (CRC_Size)crc_Size = 3
. . . . . TrCHInfo_setseq_0
. . . . . . (IntegerType)trchid = 5
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 148
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . (IntegerType)rateMatchingAttribute = 170
. . . . . . . . (CRC_Size)crc_Size = 3
. . . . TFCS
. . . . . ExplicitTFCS_Configuration
. . . . . . TFCS_ReconfAdd
. . . . . . . ctfcSize
. . . . . . . . ctfc4Bit
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 0
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 1
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 2
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 3
. . . . . . . . . . PowerOffsetInformation
. . . . dlconnectedTrCHList
. . . . TFCS
. . . TrCH_LogCHMappingList1
. . . . ulconnectedTrCHList
. . . . . TrCH_LogCHMappingList1_setseq_0
. . . . . . (IntegerType)trchid = 1
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 7
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 5
. . . . . . . . (IntegerType)rB_Identity = -12
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . TrCH_LogCHMappingList1_setseq_0
. . . . . . (IntegerType)trchid = 5
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . (IntegerType)rB_Identity = 1
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . (IntegerType)rB_Identity = 2
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . (IntegerType)rB_Identity = 3
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . (IntegerType)rB_Identity = 4
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . dlconnectedTrCHList
- Constraint:
ca_CMAC_ReconfigInfo
- BinaryMessage:
30 81 e6 02 01 ff 02 01 14 0a 01 00 30 81 da 02 02 00 88 30 00 30 61 30 46 30 21 02 01 01 30 1c 30 0e 30 0c 02 02 00 90 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 9b 0a 01 03 30 21 02 01 05 30 1c 30 0e 30 0c 02 02 00 94 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 aa 0a 01 03 30 17 30 30 14 30 03 02 01 00 30 03 02 01 01 30 03 02 01 02 30 03 02 01 03 30 6f 30 6d 30 18 02 01 01 30 13 30 11 30 0c 0a 01 00 0a 01 00 02 01 07 0a 01 05 02 01 f4 30 51 02 01 05 30 4c 30 11 30 0c 0a 01 00 0a 01 00 02 01 01 0a 01 04 02 01 01 30 11 30 0c 0a 01 00 0a 01 00 02 01 02 0a 01 04 02 01 02 30 11 30 0c 0a 01 00 0a 01 00 02 01 03 0a 01 04 02 01 03 30 11 30 0c 0a 01 00 0a 01 00 02 01 04 0a 01 04 02 01 04

- No.: 2614
- Timestamp: 10:52:40:796_0
- RFN: 4072
- Chip: 38144
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_SS_2DCH_Modify LINE 14
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 14

- No.: 2617
- Timestamp: 10:52:40:807_0
- RFN: 4074
- Chip: 3584
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB_TM_Cfg_RLC LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = -12
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_TM_RLC_Mode
. . . . . . (BooleanType)segmentationIndication = TRUE
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 144
. . . . . UL_RLC_Mode
. . . . . . UL_TM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . (BooleanType)segmentationIndication = TRUE
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = 7
. . . . (IntegerType)dLlogicalChannelIdentity = 7
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_TM_Info
- BinaryMessage:
30 25 02 01 ff 02 01 f4 0a 01 00 30 1a 30 10 30 03 01 01 ff 30 09 02 02 00 90 30 03 01 01 ff 30 06 02 01 07 02 01 07

- No.: 2621
- Timestamp: 10:52:40:820_0
- RFN: 4075
- Chip: 14848
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB_TM_Cfg_RLC LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = -12
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 f4

- No.: 2629
- Timestamp: 10:52:40:829_0
- RFN: 4076
- Chip: 11264
- Event: Start Timer
- Source: ts_RRC_ReceiveRB_SetupCmpl LINE 2
- Message Structure:
no details available
- Constraint:
t_WaitMS (13500 Ms)
- BinaryMessage:

- No.: 2638
- Timestamp: 10:52:42:494_0
- RFN: 4242
- Chip: 32768
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_IND
- Source: ts_RRC_ReceiveRB_SetupCmpl:lt_CipheringNotStartedAM_RAB LINE 4
- Message Structure:
RLC_AM_DATA_IND
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. IntegrityResult
. . (IntegrityStatus)integrityUsed = 0
. aM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "11011110110000110001011001100110"
. . . . (IntegerType)rrc_MessageSequenceNumber = 4
. . . UL_DCCH_MessageType
. . . . RadioBearerSetupComplete
. . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . IntegrityProtActivationInfo
. . . . . (IntegerType)ul_TimingAdvance = 0
. . . . . (BitStringType)start_Value[20] = "00000000000000000100"
. . . . . (IntegerType)count_C_ActivationTime = 0
. . . . . UL_CounterSynchronisationInfo
. . . . . laterNonCriticalExtensions
. . . . . . (BitStringType)radioBearerSetupComplete_r3_add_ext = 0
. . . . . . nonCriticalExtensions
- Constraint:
car_RB_SetUpCmpl
- BinaryMessage:
30 12 02 01 ff 02 01 02 0a 01 00 ef 61 8b 33 23 c8 00 00 08

- No.: 2639
- Timestamp: 10:52:42:495_0
- RFN: 4242
- Chip: 38144
- Event: Cancel Timer
- Source: ts_RRC_ReceiveRB_SetupCmpl:lt_CipheringNotStartedAM_RAB LINE 4
- Message Structure:
no details available
- Constraint:
t_WaitMS
- BinaryMessage:

- No.: 2640
- Timestamp: 10:52:42:496_0
- RFN: 4243
- Chip: 512
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ReceiveRB_SetupCmpl:lt_CipheringNotStartedAM_RAB LINE 4
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2669
- Timestamp: 10:52:42:539_0
- RFN: 4247
- Chip: 9472
- Event: Send
- PCO: Dc
- Message: RRC_DataReq
- Source: ts_TC_CloseUE_TestLoop LINE 6
- Message Structure:
RRC_DataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[-1] = -
. (SapId)sapId[1] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. CLOSEUETESTLOOP
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)tCProtocolDiscriminator[4] = '1111'B
. . (MsgType)msgType[8] = '01000000'B
. . (UE_TestLoopMode)uE_TestLoopMode[1] = '00'O
. . UE_TestLoopMode1LB_Setup
. . . (Length)iel[1] = '03'O
. . . LB_SetupRB_IE
. . . . (BitStringType)rLC_SDU_Size[16] = '0000100111111000'B
. . . . (BitStringType)spare_2[3] = '000'B
. . . . (BitStringType)rB_Identity[5] = '10100'B
. . . LB_SetupRB_IE
. . . LB_SetupRB_IE
. . . LB_SetupRB_IE
- Constraint:
ca_PS_DataReq
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 0f 40 00 03 09 f8 14

- No.: 2670
- Timestamp: 10:52:42:540_0
- RFN: 4247
- Chip: 14592
- Event: Start Timer
- Source: ts_TC_CloseUE_TestLoop LINE 6
- Message Structure:
no details available
- Constraint:
t_Dly (5000 Ms)
- BinaryMessage:

- No.: 2674
- Timestamp: 10:52:42:809_0
- RFN: 4274
- Chip: 13568
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_TC_CloseUE_TestLoop LINE 7
- Message Structure:
RRC_DataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. (START_Value)start[0] = -
. CLOSEUETESTLOOPCOMPLETE
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)tCProtocolDiscriminator[4] = '1111'B
. . (MsgType)msgType[8] = '01000001'B
- Constraint:
car_PS_UplinkDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 0f 41

- No.: 2675
- Timestamp: 10:52:42:810_0
- RFN: 4274
- Chip: 16896
- Event: Cancel Timer
- Source: ts_TC_CloseUE_TestLoop LINE 7
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 2676
- Timestamp: 10:52:42:810_1
- RFN: 4274
- Chip: 17664
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_TC_CloseUE_TestLoop LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2684
- Timestamp: 10:52:42:822_0
- RFN: 4275
- Chip: 24832
- Event: Start Timer
- Source: tc_7_2_3_19:lt_MonitorUplink LINE 1
- Message Structure:
no details available
- Constraint:
t_WaitMS (4000 Ms)
- BinaryMessage:

- No.: 2688
- Timestamp: 10:52:46:818_0
- RFN: 4675
- Chip: 10496
- Event: Timeout
- Source: tc_7_2_3_19:lt_MonitorUplink LINE 3
- Message Structure:
no details available
- Constraint:
t_WaitMS
- BinaryMessage:

- No.: 2695
- Timestamp: 10:52:46:828_0
- RFN: 4676
- Chip: 7424
- Event: Start Timer
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 8
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 2702
- Timestamp: 10:52:46:843_0
- RFN: 4677
- Chip: 27392
- Event: Timeout
- Source: tc_7_2_3_19:lt_TxAndRx LINE 6
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 2725
- Timestamp: 10:52:46:891_0
- RFN: 4682
- Chip: 22016
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000000'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000110'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001000'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'FFE665A5C5CA3452085408'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 01 05 09 0d 11 14 ff e6 65 a5 c5 ca 34 52 08 54 08

- No.: 2734
- Timestamp: 10:52:46:905_1
- RFN: 4683
- Chip: 36864
- Event: Start Timer
- Source: tc_7_2_3_19:lt_TxAndRx LINE 10
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 2735
- Timestamp: 10:52:46:905_2
- RFN: 4683
- Chip: 37632
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2740
- Timestamp: 10:52:46:919_1
- RFN: 4685
- Chip: 13568
- Event: Timeout
- Source: tc_7_2_3_19:lt_TxAndRx LINE 6
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 2742
- Timestamp: 10:52:46:922_1
- RFN: 4685
- Chip: 25856
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2747
- Timestamp: 10:52:47:074_0
- RFN: 4700
- Chip: 29952
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000000'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110011'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110011'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111001101111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111001101111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111001101111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'E6FFE6FFE6'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 00 ff e6 ff e6 ff e6 ff e6 ff e6 ff e6 ff e6 ff e6

- No.: 2751
- Timestamp: 10:52:47:079_3
- RFN: 4701
- Chip: 13824
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2756
- Timestamp: 10:52:47:094_0
- RFN: 4702
- Chip: 30976
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000001'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110011'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110011'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111001101111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111001101111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111001101111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'E6FFE6FFE6'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 08 ff e6 ff e6 ff e6 ff e6 ff e6 ff e6 ff e6 ff e6

- No.: 2760
- Timestamp: 10:52:47:100_0
- RFN: 4703
- Chip: 14848
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2765
- Timestamp: 10:52:47:114_0
- RFN: 4704
- Chip: 33024
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000010'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110011'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110011'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111001101111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111001101111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111001101111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'E6FFE6FFE6'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 10 ff e6 ff e6 ff e6 ff e6 ff e6 ff e6 ff e6 ff e6

- No.: 2769
- Timestamp: 10:52:47:120_2
- RFN: 4705
- Chip: 16384
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2774
- Timestamp: 10:52:47:134_0
- RFN: 4706
- Chip: 33792
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000011'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110011'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110011'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111001101111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111001101111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111001101111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'E6FFE6FFE6'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 18 ff e6 ff e6 ff e6 ff e6 ff e6 ff e6 ff e6 ff e6

- No.: 2778
- Timestamp: 10:52:47:140_3
- RFN: 4707
- Chip: 17664
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2783
- Timestamp: 10:52:47:155_0
- RFN: 4708
- Chip: 35072
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000100'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110011'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110011'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111001101111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111001101111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111001101111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'E6FFE6FFE6'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 20 ff e6 ff e6 ff e6 ff e6 ff e6 ff e6 ff e6 ff e6

- No.: 2787
- Timestamp: 10:52:47:160_3
- RFN: 4709
- Chip: 18432
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2792
- Timestamp: 10:52:47:175_0
- RFN: 4710
- Chip: 35584
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000101'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110011'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110011'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111001101111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111001101111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111001101111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'E6FFE6FFE6'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 28 ff e6 ff e6 ff e6 ff e6 ff e6 ff e6 ff e6 ff e6

- No.: 2796
- Timestamp: 10:52:47:181_0
- RFN: 4711
- Chip: 19968
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2799
- Timestamp: 10:52:47:193_0
- RFN: 4712
- Chip: 29440
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000110'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110011'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110011'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111001101111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111001101111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111001101111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'E6FFE6FFE6'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 30 ff e6 ff e6 ff e6 ff e6 ff e6 ff e6 ff e6 ff e6

- No.: 2803
- Timestamp: 10:52:47:200_1
- RFN: 4713
- Chip: 17152
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2808
- Timestamp: 10:52:47:215_0
- RFN: 4714
- Chip: 37888
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000111'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110011'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110011'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111001101111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111001101111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111001101111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'E6FFE6FFE6'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 38 ff e6 ff e6 ff e6 ff e6 ff e6 ff e6 ff e6 ff e6

- No.: 2812
- Timestamp: 10:52:47:223_0
- RFN: 4715
- Chip: 29696
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2815
- Timestamp: 10:52:47:233_0
- RFN: 4716
- Chip: 29440
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000001000'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110011'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110011'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111001101111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111001101111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111001101111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'E6FFE6FFE6'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 40 ff e6 ff e6 ff e6 ff e6 ff e6 ff e6 ff e6 ff e6

- No.: 2819
- Timestamp: 10:52:47:244_0
- RFN: 4717
- Chip: 30208
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2822
- Timestamp: 10:52:47:254_0
- RFN: 4718
- Chip: 30464
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000001001'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110011'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110011'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111001101111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111001101111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111001101111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'E6FFE6FFE6'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 48 ff e6 ff e6 ff e6 ff e6 ff e6 ff e6 ff e6 ff e6

- No.: 2826
- Timestamp: 10:52:47:260_1
- RFN: 4719
- Chip: 14592
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2831
- Timestamp: 10:52:47:274_0
- RFN: 4720
- Chip: 31232
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000001010'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110011'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110011'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111001101111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111001101111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111001101111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'E6FFE6FFE6'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 50 ff e6 ff e6 ff e6 ff e6 ff e6 ff e6 ff e6 ff e6

- No.: 2835
- Timestamp: 10:52:47:280_2
- RFN: 4721
- Chip: 14592
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2840
- Timestamp: 10:52:47:294_0
- RFN: 4722
- Chip: 32000
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000001011'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110011'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110011'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111001101111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111001101111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111001101111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'E6FFE6FFE6'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 58 ff e6 ff e6 ff e6 ff e6 ff e6 ff e6 ff e6 ff e6

- No.: 2844
- Timestamp: 10:52:47:300_3
- RFN: 4723
- Chip: 16128
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2849
- Timestamp: 10:52:47:315_0
- RFN: 4724
- Chip: 33536
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000001100'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110011'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110011'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111001101111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111001101111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111001101111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'E6FFE6FFE6'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 60 ff e6 ff e6 ff e6 ff e6 ff e6 ff e6 ff e6 ff e6

- No.: 2853
- Timestamp: 10:52:47:321_1
- RFN: 4725
- Chip: 18176
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2858
- Timestamp: 10:52:47:336_0
- RFN: 4727
- Chip: 256
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000001101'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110011'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110011'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111001101111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111001101111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111001101111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'E6FFE6FFE6'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 68 ff e6 ff e6 ff e6 ff e6 ff e6 ff e6 ff e6 ff e6

- No.: 2862
- Timestamp: 10:52:47:344_1
- RFN: 4727
- Chip: 30720
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2865
- Timestamp: 10:52:47:354_0
- RFN: 4728
- Chip: 29696
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000001110'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110011'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110011'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111001101111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111001101111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111001101111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'E6FFE6FFE6'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 70 ff e6 ff e6 ff e6 ff e6 ff e6 ff e6 ff e6 ff e6

- No.: 2869
- Timestamp: 10:52:47:359_3
- RFN: 4729
- Chip: 13056
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2874
- Timestamp: 10:52:47:374_0
- RFN: 4730
- Chip: 30464
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000001111'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110011'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110011'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111001101111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111001101111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111001101111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'E6FFE6FFE6'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 78 ff e6 ff e6 ff e6 ff e6 ff e6 ff e6 ff e6 ff e6

- No.: 2878
- Timestamp: 10:52:47:380_0
- RFN: 4731
- Chip: 13824
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2883
- Timestamp: 10:52:47:394_0
- RFN: 4732
- Chip: 31744
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000010000'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110011'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110011'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111001101111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111001101111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111001101111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'E6FFE6FFE6'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 80 ff e6 ff e6 ff e6 ff e6 ff e6 ff e6 ff e6 ff e6

- No.: 2887
- Timestamp: 10:52:47:400_1
- RFN: 4733
- Chip: 15360
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2892
- Timestamp: 10:52:47:414_0
- RFN: 4734
- Chip: 32768
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000010001'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110011'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110011'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111001101111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111001101111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111001101111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'E6FFE6FFE6'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 88 ff e6 ff e6 ff e6 ff e6 ff e6 ff e6 ff e6 ff e6

- No.: 2896
- Timestamp: 10:52:47:420_3
- RFN: 4735
- Chip: 17408
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2901
- Timestamp: 10:52:47:436_0
- RFN: 4736
- Chip: 37888
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000010010'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110011'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110011'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111001101111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111001101111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111001101111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'E6FFE6FFE6'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 90 ff e6 ff e6 ff e6 ff e6 ff e6 ff e6 ff e6 ff e6

- No.: 2905
- Timestamp: 10:52:47:443_0
- RFN: 4737
- Chip: 29952
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2908
- Timestamp: 10:52:47:453_0
- RFN: 4738
- Chip: 28672
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000010011'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110011'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1111111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110011'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111111111110011'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111111111110011'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111111111110011'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = 'FFE6FFE6FF'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 99 1e ff e6 ff e6 ff e6 ff e6 ff e6 ff e6 ff e6 ff

- No.: 2912
- Timestamp: 10:52:47:459_1
- RFN: 4739
- Chip: 12288
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2917
- Timestamp: 10:52:47:473_0
- RFN: 4740
- Chip: 29440
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000010100'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101001010110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101001010110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101001010110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'A565A565A5'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 a0 65 a5 65 a5 65 a5 65 a5 65 a5 65 a5 65 a5 65 a5

- No.: 2921
- Timestamp: 10:52:47:479_2
- RFN: 4741
- Chip: 13824
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2926
- Timestamp: 10:52:47:494_0
- RFN: 4742
- Chip: 34560
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000010101'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101001010110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101001010110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101001010110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'A565A565A5'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 a8 65 a5 65 a5 65 a5 65 a5 65 a5 65 a5 65 a5 65 a5

- No.: 2930
- Timestamp: 10:52:47:501_0
- RFN: 4743
- Chip: 19200
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2935
- Timestamp: 10:52:47:516_0
- RFN: 4745
- Chip: 2048
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000010110'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101001010110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101001010110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101001010110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'A565A565A5'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 b0 65 a5 65 a5 65 a5 65 a5 65 a5 65 a5 65 a5 65 a5

- No.: 2939
- Timestamp: 10:52:47:524_3
- RFN: 4745
- Chip: 34304
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2942
- Timestamp: 10:52:47:534_0
- RFN: 4746
- Chip: 33280
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000010111'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101001010110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101001010110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101001010110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'A565A565A5'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 b8 65 a5 65 a5 65 a5 65 a5 65 a5 65 a5 65 a5 65 a5

- No.: 2946
- Timestamp: 10:52:47:540_1
- RFN: 4747
- Chip: 17152
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2951
- Timestamp: 10:52:47:555_0
- RFN: 4748
- Chip: 34048
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000011000'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101001010110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101001010110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101001010110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'A565A565A5'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 c0 65 a5 65 a5 65 a5 65 a5 65 a5 65 a5 65 a5 65 a5

- No.: 2955
- Timestamp: 10:52:47:561_1
- RFN: 4749
- Chip: 17664
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2960
- Timestamp: 10:52:47:575_0
- RFN: 4750
- Chip: 34560
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000011001'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101001010110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101001010110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101001010110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'A565A565A5'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 c8 65 a5 65 a5 65 a5 65 a5 65 a5 65 a5 65 a5 65 a5

- No.: 2964
- Timestamp: 10:52:47:581_3
- RFN: 4751
- Chip: 19200
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2969
- Timestamp: 10:52:47:597_0
- RFN: 4753
- Chip: 1792
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000011010'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101001010110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101001010110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101001010110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'A565A565A5'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 d0 65 a5 65 a5 65 a5 65 a5 65 a5 65 a5 65 a5 65 a5

- No.: 2973
- Timestamp: 10:52:47:603_2
- RFN: 4753
- Chip: 26112
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2976
- Timestamp: 10:52:47:614_0
- RFN: 4754
- Chip: 31488
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000011011'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101001010110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101001010110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101001010110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'A565A565A5'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 d8 65 a5 65 a5 65 a5 65 a5 65 a5 65 a5 65 a5 65 a5

- No.: 2980
- Timestamp: 10:52:47:620_2
- RFN: 4755
- Chip: 15104
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2985
- Timestamp: 10:52:47:634_0
- RFN: 4756
- Chip: 32256
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000011100'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101001010110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101001010110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101001010110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'A565A565A5'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 e0 65 a5 65 a5 65 a5 65 a5 65 a5 65 a5 65 a5 65 a5

- No.: 2989
- Timestamp: 10:52:47:640_3
- RFN: 4757
- Chip: 15872
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2994
- Timestamp: 10:52:47:654_0
- RFN: 4758
- Chip: 32768
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000011101'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101001010110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101001010110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101001010110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'A565A565A5'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 e8 65 a5 65 a5 65 a5 65 a5 65 a5 65 a5 65 a5 65 a5

- No.: 2998
- Timestamp: 10:52:47:660_3
- RFN: 4759
- Chip: 17152
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3003
- Timestamp: 10:52:47:676_0
- RFN: 4760
- Chip: 37888
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000011110'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101001010110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101001010110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101001010110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'A565A565A5'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 f0 65 a5 65 a5 65 a5 65 a5 65 a5 65 a5 65 a5 65 a5

- No.: 3007
- Timestamp: 10:52:47:684_1
- RFN: 4761
- Chip: 32256
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3010
- Timestamp: 10:52:47:695_0
- RFN: 4762
- Chip: 35584
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000011111'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101001010110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101001010110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101001010110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'A565A565A5'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 f8 65 a5 65 a5 65 a5 65 a5 65 a5 65 a5 65 a5 65 a5

- No.: 3014
- Timestamp: 10:52:47:701_1
- RFN: 4763
- Chip: 19200
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3019
- Timestamp: 10:52:47:716_0
- RFN: 4764
- Chip: 37632
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000100000'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101001010110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101001010110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101001010110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'A565A565A5'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 00 65 a5 65 a5 65 a5 65 a5 65 a5 65 a5 65 a5 65 a5

- No.: 3023
- Timestamp: 10:52:47:721_3
- RFN: 4765
- Chip: 22784
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3028
- Timestamp: 10:52:47:736_0
- RFN: 4767
- Chip: 512
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000100001'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101001010110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101001010110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101001010110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'A565A565A5'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 08 65 a5 65 a5 65 a5 65 a5 65 a5 65 a5 65 a5 65 a5

- No.: 3032
- Timestamp: 10:52:47:744_0
- RFN: 4767
- Chip: 30976
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3035
- Timestamp: 10:52:47:753_0
- RFN: 4768
- Chip: 29696
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000100010'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101001010110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101001010110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101001010110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'A565A565A5'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 10 65 a5 65 a5 65 a5 65 a5 65 a5 65 a5 65 a5 65 a5

- No.: 3039
- Timestamp: 10:52:47:759_3
- RFN: 4769
- Chip: 13568
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3044
- Timestamp: 10:52:47:774_0
- RFN: 4770
- Chip: 30720
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000100011'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101001010110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101001010110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101001010110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'A565A565A5'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 18 65 a5 65 a5 65 a5 65 a5 65 a5 65 a5 65 a5 65 a5

- No.: 3048
- Timestamp: 10:52:47:780_0
- RFN: 4771
- Chip: 15104
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3053
- Timestamp: 10:52:47:795_0
- RFN: 4772
- Chip: 36352
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000100100'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101001010110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101001010110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101001010110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'A565A565A5'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 20 65 a5 65 a5 65 a5 65 a5 65 a5 65 a5 65 a5 65 a5

- No.: 3057
- Timestamp: 10:52:47:801_1
- RFN: 4773
- Chip: 19968
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3060
- Timestamp: 10:52:47:813_0
- RFN: 4774
- Chip: 27648
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000100101'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101001010110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101001010110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101001010110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'A565A565A5'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 28 65 a5 65 a5 65 a5 65 a5 65 a5 65 a5 65 a5 65 a5

- No.: 3064
- Timestamp: 10:52:47:818_3
- RFN: 4775
- Chip: 11264
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3069
- Timestamp: 10:52:47:833_0
- RFN: 4776
- Chip: 27904
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000100110'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101001010110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101001010110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101001010110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'A565A565A5'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 30 65 a5 65 a5 65 a5 65 a5 65 a5 65 a5 65 a5 65 a5

- No.: 3073
- Timestamp: 10:52:47:838_3
- RFN: 4777
- Chip: 11520
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3078
- Timestamp: 10:52:47:853_0
- RFN: 4778
- Chip: 29184
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000100111'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0110010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '011001011010010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '011001011010010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '011001011010010'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = '65A565A565'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 39 1e 65 a5 65 a5 65 a5 65 a5 65 a5 65 a5 65 a5 65

- No.: 3082
- Timestamp: 10:52:47:859_2
- RFN: 4779
- Chip: 14080
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3087
- Timestamp: 10:52:47:875_0
- RFN: 4780
- Chip: 34304
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000101000'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100101'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100101'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110010101100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110010101100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110010101100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'CAC5CAC5CA'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 40 c5 ca c5 ca c5 ca c5 ca c5 ca c5 ca c5 ca c5 ca

- No.: 3091
- Timestamp: 10:52:47:881_2
- RFN: 4781
- Chip: 18688
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3096
- Timestamp: 10:52:47:896_0
- RFN: 4782
- Chip: 36096
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000101001'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100101'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100101'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110010101100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110010101100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110010101100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'CAC5CAC5CA'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 48 c5 ca c5 ca c5 ca c5 ca c5 ca c5 ca c5 ca c5 ca

- No.: 3100
- Timestamp: 10:52:47:901_3
- RFN: 4783
- Chip: 19712
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3105
- Timestamp: 10:52:47:916_0
- RFN: 4784
- Chip: 36352
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000101010'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100101'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100101'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110010101100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110010101100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110010101100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'CAC5CAC5CA'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 50 c5 ca c5 ca c5 ca c5 ca c5 ca c5 ca c5 ca c5 ca

- No.: 3109
- Timestamp: 10:52:47:921_3
- RFN: 4785
- Chip: 20480
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3114
- Timestamp: 10:52:47:936_0
- RFN: 4786
- Chip: 37120
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000101011'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100101'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100101'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110010101100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110010101100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110010101100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'CAC5CAC5CA'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 58 c5 ca c5 ca c5 ca c5 ca c5 ca c5 ca c5 ca c5 ca

- No.: 3118
- Timestamp: 10:52:47:941_3
- RFN: 4787
- Chip: 20480
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3121
- Timestamp: 10:52:47:953_0
- RFN: 4788
- Chip: 27648
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000101100'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100101'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100101'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110010101100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110010101100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110010101100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'CAC5CAC5CA'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 60 c5 ca c5 ca c5 ca c5 ca c5 ca c5 ca c5 ca c5 ca

- No.: 3125
- Timestamp: 10:52:47:959_3
- RFN: 4789
- Chip: 12544
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3130
- Timestamp: 10:52:47:974_0
- RFN: 4790
- Chip: 32768
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000101101'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100101'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100101'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110010101100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110010101100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110010101100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'CAC5CAC5CA'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 68 c5 ca c5 ca c5 ca c5 ca c5 ca c5 ca c5 ca c5 ca

- No.: 3134
- Timestamp: 10:52:47:980_3
- RFN: 4791
- Chip: 16640
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3139
- Timestamp: 10:52:47:995_0
- RFN: 4792
- Chip: 34304
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000101110'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100101'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100101'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110010101100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110010101100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110010101100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'CAC5CAC5CA'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 70 c5 ca c5 ca c5 ca c5 ca c5 ca c5 ca c5 ca c5 ca

- No.: 3143
- Timestamp: 10:52:48:000_3
- RFN: 4793
- Chip: 17664
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3148
- Timestamp: 10:52:48:015_0
- RFN: 4794
- Chip: 34560
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000101111'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100101'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100101'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110010101100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110010101100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110010101100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'CAC5CAC5CA'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 78 c5 ca c5 ca c5 ca c5 ca c5 ca c5 ca c5 ca c5 ca

- No.: 3152
- Timestamp: 10:52:48:021_2
- RFN: 4795
- Chip: 20224
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3157
- Timestamp: 10:52:48:037_0
- RFN: 4797
- Chip: 3328
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000110000'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100101'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100101'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110010101100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110010101100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110010101100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'CAC5CAC5CA'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 80 c5 ca c5 ca c5 ca c5 ca c5 ca c5 ca c5 ca c5 ca

- No.: 3161
- Timestamp: 10:52:48:044_3
- RFN: 4797
- Chip: 33280
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3164
- Timestamp: 10:52:48:054_0
- RFN: 4798
- Chip: 32256
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000110001'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100101'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100101'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110010101100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110010101100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110010101100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'CAC5CAC5CA'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 88 c5 ca c5 ca c5 ca c5 ca c5 ca c5 ca c5 ca c5 ca

- No.: 3168
- Timestamp: 10:52:48:060_1
- RFN: 4799
- Chip: 16128
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3173
- Timestamp: 10:52:48:074_0
- RFN: 4800
- Chip: 32512
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000110010'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100101'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100101'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110010101100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110010101100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110010101100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'CAC5CAC5CA'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 90 c5 ca c5 ca c5 ca c5 ca c5 ca c5 ca c5 ca c5 ca

- No.: 3177
- Timestamp: 10:52:48:080_2
- RFN: 4801
- Chip: 16640
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3182
- Timestamp: 10:52:48:094_0
- RFN: 4802
- Chip: 33536
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000110011'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100101'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100101'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110010101100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110010101100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110010101100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'CAC5CAC5CA'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 98 c5 ca c5 ca c5 ca c5 ca c5 ca c5 ca c5 ca c5 ca

- No.: 3186
- Timestamp: 10:52:48:100_3
- RFN: 4803
- Chip: 18944
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3191
- Timestamp: 10:52:48:116_0
- RFN: 4805
- Chip: 1024
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000110100'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100101'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100101'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110010101100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110010101100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110010101100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'CAC5CAC5CA'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 a0 c5 ca c5 ca c5 ca c5 ca c5 ca c5 ca c5 ca c5 ca

- No.: 3195
- Timestamp: 10:52:48:122_1
- RFN: 4805
- Chip: 24576
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3200
- Timestamp: 10:52:48:136_0
- RFN: 4807
- Chip: 2560
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000110101'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100101'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100101'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110010101100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110010101100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110010101100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'CAC5CAC5CA'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 a8 c5 ca c5 ca c5 ca c5 ca c5 ca c5 ca c5 ca c5 ca

- No.: 3204
- Timestamp: 10:52:48:144_3
- RFN: 4807
- Chip: 34048
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3207
- Timestamp: 10:52:48:154_0
- RFN: 4808
- Chip: 34304
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000110110'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100101'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100101'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110010101100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110010101100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110010101100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'CAC5CAC5CA'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 b0 c5 ca c5 ca c5 ca c5 ca c5 ca c5 ca c5 ca c5 ca

- No.: 3211
- Timestamp: 10:52:48:160_3
- RFN: 4809
- Chip: 18432
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3216
- Timestamp: 10:52:48:175_0
- RFN: 4810
- Chip: 36352
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000110111'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100101'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100101'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110010101100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110010101100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110010101100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'CAC5CAC5CA'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 b8 c5 ca c5 ca c5 ca c5 ca c5 ca c5 ca c5 ca c5 ca

- No.: 3220
- Timestamp: 10:52:48:181_3
- RFN: 4811
- Chip: 19712
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3223
- Timestamp: 10:52:48:193_0
- RFN: 4812
- Chip: 27136
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000111000'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100101'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100101'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110010101100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110010101100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110010101100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'CAC5CAC5CA'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 c0 c5 ca c5 ca c5 ca c5 ca c5 ca c5 ca c5 ca c5 ca

- No.: 3227
- Timestamp: 10:52:48:200_3
- RFN: 4813
- Chip: 15872
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3232
- Timestamp: 10:52:48:217_0
- RFN: 4815
- Chip: 1792
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000111001'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100101'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100101'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110010101100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110010101100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110010101100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'CAC5CAC5CA'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 c8 c5 ca c5 ca c5 ca c5 ca c5 ca c5 ca c5 ca c5 ca

- No.: 3236
- Timestamp: 10:52:48:223_1
- RFN: 4815
- Chip: 25600
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3241
- Timestamp: 10:52:48:239_0
- RFN: 4817
- Chip: 11264
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000111010'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100101'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100101'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110010101100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110010101100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110010101100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'CAC5CAC5CA'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 d0 c5 ca c5 ca c5 ca c5 ca c5 ca c5 ca c5 ca c5 ca

- No.: 3245
- Timestamp: 10:52:48:247_3
- RFN: 4818
- Chip: 4608
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3248
- Timestamp: 10:52:48:256_0
- RFN: 4819
- Chip: 1280
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000111011'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100101'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100101'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110001011100101'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110001011100101'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110001011100101'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = 'C5CAC5CAC5'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 d9 1e c5 ca c5 ca c5 ca c5 ca c5 ca c5 ca c5 ca c5

- No.: 3252
- Timestamp: 10:52:48:264_2
- RFN: 4819
- Chip: 32000
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3255
- Timestamp: 10:52:48:274_0
- RFN: 4820
- Chip: 30976
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000111100'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101001'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101001'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010100100011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010100100011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010100100011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '5234523452'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 e0 34 52 34 52 34 52 34 52 34 52 34 52 34 52 34 52

- No.: 3259
- Timestamp: 10:52:48:280_1
- RFN: 4821
- Chip: 14592
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3264
- Timestamp: 10:52:48:294_0
- RFN: 4822
- Chip: 31488
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000111101'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101001'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101001'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010100100011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010100100011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010100100011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '5234523452'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 e8 34 52 34 52 34 52 34 52 34 52 34 52 34 52 34 52

- No.: 3268
- Timestamp: 10:52:48:300_3
- RFN: 4823
- Chip: 16384
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3273
- Timestamp: 10:52:48:315_0
- RFN: 4824
- Chip: 36608
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000111110'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101001'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101001'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010100100011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010100100011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010100100011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '5234523452'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 f0 34 52 34 52 34 52 34 52 34 52 34 52 34 52 34 52

- No.: 3277
- Timestamp: 10:52:48:321_3
- RFN: 4825
- Chip: 20480
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3280
- Timestamp: 10:52:48:333_0
- RFN: 4826
- Chip: 28160
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000111111'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101001'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101001'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010100100011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010100100011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010100100011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '5234523452'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 f8 34 52 34 52 34 52 34 52 34 52 34 52 34 52 34 52

- No.: 3284
- Timestamp: 10:52:48:339_1
- RFN: 4827
- Chip: 11776
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3289
- Timestamp: 10:52:48:353_0
- RFN: 4828
- Chip: 29440
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001000000'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101001'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101001'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010100100011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010100100011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010100100011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '5234523452'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 00 34 52 34 52 34 52 34 52 34 52 34 52 34 52 34 52

- No.: 3293
- Timestamp: 10:52:48:359_3
- RFN: 4829
- Chip: 13824
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3298
- Timestamp: 10:52:48:374_0
- RFN: 4830
- Chip: 30720
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001000001'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101001'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101001'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010100100011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010100100011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010100100011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '5234523452'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 08 34 52 34 52 34 52 34 52 34 52 34 52 34 52 34 52

- No.: 3302
- Timestamp: 10:52:48:380_0
- RFN: 4831
- Chip: 15360
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3307
- Timestamp: 10:52:48:394_0
- RFN: 4832
- Chip: 32512
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001000010'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101001'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101001'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010100100011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010100100011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010100100011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '5234523452'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 10 34 52 34 52 34 52 34 52 34 52 34 52 34 52 34 52

- No.: 3311
- Timestamp: 10:52:48:400_2
- RFN: 4833
- Chip: 17664
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3316
- Timestamp: 10:52:48:415_0
- RFN: 4834
- Chip: 37376
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001000011'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101001'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101001'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010100100011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010100100011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010100100011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '5234523452'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 18 34 52 34 52 34 52 34 52 34 52 34 52 34 52 34 52

- No.: 3320
- Timestamp: 10:52:48:423_0
- RFN: 4835
- Chip: 29440
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3323
- Timestamp: 10:52:48:433_0
- RFN: 4836
- Chip: 28672
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001000100'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101001'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101001'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010100100011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010100100011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010100100011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '5234523452'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 20 34 52 34 52 34 52 34 52 34 52 34 52 34 52 34 52

- No.: 3327
- Timestamp: 10:52:48:439_1
- RFN: 4837
- Chip: 12800
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3332
- Timestamp: 10:52:48:453_0
- RFN: 4838
- Chip: 29696
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001000101'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101001'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101001'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010100100011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010100100011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010100100011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '5234523452'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 28 34 52 34 52 34 52 34 52 34 52 34 52 34 52 34 52

- No.: 3336
- Timestamp: 10:52:48:459_1
- RFN: 4839
- Chip: 13568
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3341
- Timestamp: 10:52:48:473_0
- RFN: 4840
- Chip: 30208
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001000110'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101001'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101001'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010100100011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010100100011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010100100011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '5234523452'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 34 34 52 34 52 34 52 34 52 34 52 34 52 34 52 34 52

- No.: 3347
- Timestamp: 10:52:48:490_1
- RFN: 4842
- Chip: 19200
- Event: Start Timer
- Source: tc_7_2_3_19:lt_CheckPollBit LINE 5
- Message Structure:
no details available
- Constraint:
t_LowerBound (1800 Ms)
- BinaryMessage:

- No.: 3348
- Timestamp: 10:52:48:492_0
- RFN: 4842
- Chip: 20736
- Event: Start Timer
- Source: tc_7_2_3_19:lt_CheckPollBit LINE 5
- Message Structure:
no details available
- Constraint:
t_UpperBound (2200 Ms)
- BinaryMessage:

- No.: 3350
- Timestamp: 10:52:48:492_2
- RFN: 4842
- Chip: 22528
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3353
- Timestamp: 10:52:48:505_0
- RFN: 4843
- Chip: 31744
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001000111'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101001'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101001'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010100100011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010100100011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010100100011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '5234523452'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 38 34 52 34 52 34 52 34 52 34 52 34 52 34 52 34 52

- No.: 3357
- Timestamp: 10:52:48:511_0
- RFN: 4844
- Chip: 17152
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3360
- Timestamp: 10:52:48:520_0
- RFN: 4845
- Chip: 13568
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001001000'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101001'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101001'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010100100011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010100100011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010100100011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '5234523452'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 40 34 52 34 52 34 52 34 52 34 52 34 52 34 52 34 52

- No.: 3364
- Timestamp: 10:52:48:528_2
- RFN: 4846
- Chip: 7680
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3367
- Timestamp: 10:52:48:537_0
- RFN: 4847
- Chip: 4096
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001001001'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101001'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101001'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010100100011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010100100011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010100100011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '5234523452'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 48 34 52 34 52 34 52 34 52 34 52 34 52 34 52 34 52

- No.: 3371
- Timestamp: 10:52:48:545_3
- RFN: 4847
- Chip: 35072
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3374
- Timestamp: 10:52:48:555_0
- RFN: 4848
- Chip: 33536
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001001010'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101001'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101001'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010100100011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010100100011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010100100011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '5234523452'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 50 34 52 34 52 34 52 34 52 34 52 34 52 34 52 34 52

- No.: 3378
- Timestamp: 10:52:48:561_2
- RFN: 4849
- Chip: 18944
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3383
- Timestamp: 10:52:48:576_0
- RFN: 4850
- Chip: 36352
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001001011'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101001'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101001'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010100100011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010100100011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010100100011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '5234523452'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 58 34 52 34 52 34 52 34 52 34 52 34 52 34 52 34 52

- No.: 3387
- Timestamp: 10:52:48:582_0
- RFN: 4851
- Chip: 21504
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3390
- Timestamp: 10:52:48:594_0
- RFN: 4852
- Chip: 30464
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001001100'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101001'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101001'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010100100011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010100100011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010100100011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '5234523452'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 60 34 52 34 52 34 52 34 52 34 52 34 52 34 52 34 52

- No.: 3394
- Timestamp: 10:52:48:600_1
- RFN: 4853
- Chip: 14848
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3399
- Timestamp: 10:52:48:614_0
- RFN: 4854
- Chip: 32000
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001001101'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101001'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101001'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010100100011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010100100011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010100100011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '5234523452'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 68 34 52 34 52 34 52 34 52 34 52 34 52 34 52 34 52

- No.: 3403
- Timestamp: 10:52:48:620_2
- RFN: 4855
- Chip: 16384
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3408
- Timestamp: 10:52:48:635_0
- RFN: 4856
- Chip: 33792
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001001110'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101001'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101001'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010100100011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010100100011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010100100011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '5234523452'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 70 34 52 34 52 34 52 34 52 34 52 34 52 34 52 34 52

- No.: 3412
- Timestamp: 10:52:48:640_3
- RFN: 4857
- Chip: 17408
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3417
- Timestamp: 10:52:48:655_0
- RFN: 4858
- Chip: 35072
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001001111'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101001'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101001'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '001101000101001'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '001101000101001'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '001101000101001'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '3452345234'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 79 1e 34 52 34 52 34 52 34 52 34 52 34 52 34 52 34

- No.: 3421
- Timestamp: 10:52:48:661_0
- RFN: 4859
- Chip: 18944
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3426
- Timestamp: 10:52:48:675_0
- RFN: 4860
- Chip: 35328
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001010000'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010101000000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010101000000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010101000000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '5408540854'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 80 08 54 08 54 08 54 08 54 08 54 08 54 08 54 08 54

- No.: 3430
- Timestamp: 10:52:48:681_0
- RFN: 4861
- Chip: 18944
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3435
- Timestamp: 10:52:48:696_0
- RFN: 4863
- Chip: 1024
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001010001'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010101000000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010101000000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010101000000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '5408540854'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 88 08 54 08 54 08 54 08 54 08 54 08 54 08 54 08 54

- No.: 3439
- Timestamp: 10:52:48:704_3
- RFN: 4863
- Chip: 33536
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3442
- Timestamp: 10:52:48:714_0
- RFN: 4864
- Chip: 33536
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001010010'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010101000000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010101000000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010101000000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '5408540854'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 90 08 54 08 54 08 54 08 54 08 54 08 54 08 54 08 54

- No.: 3446
- Timestamp: 10:52:48:720_2
- RFN: 4865
- Chip: 17408
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3451
- Timestamp: 10:52:48:735_0
- RFN: 4866
- Chip: 35072
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001010011'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010101000000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010101000000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010101000000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '5408540854'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 98 08 54 08 54 08 54 08 54 08 54 08 54 08 54 08 54

- No.: 3455
- Timestamp: 10:52:48:741_0
- RFN: 4867
- Chip: 19200
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3460
- Timestamp: 10:52:48:755_0
- RFN: 4868
- Chip: 35840
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001010100'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010101000000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010101000000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010101000000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '5408540854'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 a0 08 54 08 54 08 54 08 54 08 54 08 54 08 54 08 54

- No.: 3464
- Timestamp: 10:52:48:761_1
- RFN: 4869
- Chip: 29696
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3467
- Timestamp: 10:52:48:773_0
- RFN: 4870
- Chip: 29696
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001010101'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010101000000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010101000000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010101000000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '5408540854'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 a8 08 54 08 54 08 54 08 54 08 54 08 54 08 54 08 54

- No.: 3471
- Timestamp: 10:52:48:779_2
- RFN: 4871
- Chip: 13824
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3476
- Timestamp: 10:52:48:794_0
- RFN: 4872
- Chip: 31744
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001010110'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010101000000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010101000000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010101000000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '5408540854'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 b0 08 54 08 54 08 54 08 54 08 54 08 54 08 54 08 54

- No.: 3480
- Timestamp: 10:52:48:799_3
- RFN: 4873
- Chip: 15872
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3485
- Timestamp: 10:52:48:815_0
- RFN: 4874
- Chip: 32256
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001010111'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010101000000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010101000000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010101000000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '5408540854'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 b8 08 54 08 54 08 54 08 54 08 54 08 54 08 54 08 54

- No.: 3489
- Timestamp: 10:52:48:820_3
- RFN: 4875
- Chip: 15872
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3494
- Timestamp: 10:52:48:835_0
- RFN: 4876
- Chip: 32768
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001011000'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010101000000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010101000000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010101000000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '5408540854'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 c0 08 54 08 54 08 54 08 54 08 54 08 54 08 54 08 54

- No.: 3498
- Timestamp: 10:52:48:841_0
- RFN: 4877
- Chip: 16640
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3503
- Timestamp: 10:52:48:855_0
- RFN: 4878
- Chip: 33280
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001011001'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010101000000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010101000000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010101000000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '5408540854'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 c8 08 54 08 54 08 54 08 54 08 54 08 54 08 54 08 54

- No.: 3507
- Timestamp: 10:52:48:861_0
- RFN: 4879
- Chip: 16896
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3512
- Timestamp: 10:52:48:875_0
- RFN: 4880
- Chip: 33536
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001011010'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010101000000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010101000000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010101000000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '5408540854'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 d0 08 54 08 54 08 54 08 54 08 54 08 54 08 54 08 54

- No.: 3516
- Timestamp: 10:52:48:881_0
- RFN: 4881
- Chip: 17664
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3521
- Timestamp: 10:52:48:895_0
- RFN: 4882
- Chip: 34304
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001011011'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010101000000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010101000000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010101000000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '5408540854'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 d8 08 54 08 54 08 54 08 54 08 54 08 54 08 54 08 54

- No.: 3525
- Timestamp: 10:52:48:901_2
- RFN: 4883
- Chip: 19200
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3530
- Timestamp: 10:52:48:916_0
- RFN: 4885
- Chip: 1024
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001011100'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010101000000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010101000000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010101000000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '5408540854'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 e0 08 54 08 54 08 54 08 54 08 54 08 54 08 54 08 54

- No.: 3534
- Timestamp: 10:52:48:924_2
- RFN: 4885
- Chip: 32000
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3537
- Timestamp: 10:52:48:934_0
- RFN: 4886
- Chip: 31488
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001011101'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010101000000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010101000000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010101000000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '5408540854'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 e8 08 54 08 54 08 54 08 54 08 54 08 54 08 54 08 54

- No.: 3541
- Timestamp: 10:52:48:940_1
- RFN: 4887
- Chip: 15360
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3546
- Timestamp: 10:52:48:954_0
- RFN: 4888
- Chip: 31744
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001011110'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010101000000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010101000000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010101000000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '5408540854'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 f0 08 54 08 54 08 54 08 54 08 54 08 54 08 54 08 54

- No.: 3550
- Timestamp: 10:52:48:960_2
- RFN: 4889
- Chip: 15872
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3555
- Timestamp: 10:52:48:974_0
- RFN: 4890
- Chip: 33024
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001011111'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010101000000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010101000000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010101000000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '5408540854'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 f8 08 54 08 54 08 54 08 54 08 54 08 54 08 54 08 54

- No.: 3559
- Timestamp: 10:52:48:980_2
- RFN: 4891
- Chip: 16896
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3564
- Timestamp: 10:52:48:995_0
- RFN: 4892
- Chip: 33792
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001100000'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010101000000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010101000000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010101000000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '5408540854'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 00 08 54 08 54 08 54 08 54 08 54 08 54 08 54 08 54

- No.: 3568
- Timestamp: 10:52:49:000_3
- RFN: 4893
- Chip: 17664
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3573
- Timestamp: 10:52:49:015_0
- RFN: 4894
- Chip: 34048
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001100001'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010101000000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010101000000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010101000000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '5408540854'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 08 08 54 08 54 08 54 08 54 08 54 08 54 08 54 08 54

- No.: 3577
- Timestamp: 10:52:49:020_3
- RFN: 4895
- Chip: 18176
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3582
- Timestamp: 10:52:49:035_0
- RFN: 4896
- Chip: 36864
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001100010'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010101000000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010101000000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010101000000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '5408540854'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 10 08 54 08 54 08 54 08 54 08 54 08 54 08 54 08 54

- No.: 3586
- Timestamp: 10:52:49:043_0
- RFN: 4897
- Chip: 30720
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3589
- Timestamp: 10:52:49:054_0
- RFN: 4898
- Chip: 31232
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001100011'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '000010000101010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '000010000101010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '000010000101010'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '0854085408'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 19 1e 08 54 08 54 08 54 08 54 08 54 08 54 08 54 08

- No.: 3593
- Timestamp: 10:52:49:060_0
- RFN: 4899
- Chip: 15360
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3598
- Timestamp: 10:52:50:287_1
- RFN: 5022
- Chip: 6656
- Event: Timeout
- Source: tc_7_2_3_19:lt_TxAndRx LINE 1
- Message Structure:
no details available
- Constraint:
t_LowerBound
- BinaryMessage:

- No.: 3600
- Timestamp: 10:52:50:290_1
- RFN: 5022
- Chip: 17152
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3605
- Timestamp: 10:52:50:473_0
- RFN: 5040
- Chip: 26624
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001100011'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0101010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '000010000101010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '000010000101010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '000010000101010'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '0854085408'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 1d 1e 08 54 08 54 08 54 08 54 08 54 08 54 08 54 08

- No.: 3611
- Timestamp: 10:52:50:487_1
- RFN: 5042
- Chip: 4864
- Event: Start Timer
- Source: tc_7_2_3_19:lt_CheckPollBit LINE 7
- Message Structure:
no details available
- Constraint:
t_Dly (20000 Ms)
- BinaryMessage:

- No.: 3613
- Timestamp: 10:52:50:490_1
- RFN: 5042
- Chip: 16896
- Event: Cancel Timer
- Source: tc_7_2_3_19:lt_CheckPollBit LINE 8
- Message Structure:
no details available
- Constraint:
t_UpperBound
- BinaryMessage:

- No.: 3614
- Timestamp: 10:52:50:496_0
- RFN: 5043
- Chip: 1536
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: tc_7_2_3_19:lt_CheckPollBit LINE 9
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. STATUS_PDU
. . (DC_Field)dC_Field[1] = '0'B
. . (CtrlPDU_Type)type[3] = '000'B
. . SuperFields
. . . SUFI_WindowSize
. . . SUFI_List
. . . SUFI_RList
. . . SUFI_Bitmap
. . . SUFI_MRW
. . . SUFI_MRW_ACK
. . . SUFI_NoMore
. . . SUFI_Ack
. . . . (SUFI_Type)type[4] = '0010'B
. . . . (AM_SeqNum)lsn[12] = '000001100100'B
. . (HexStringType)superFieldsAndPadRx[-1] = -
. . (Padding)paddingTx[-1] = '0000000000000000000000000000000'H
- Constraint:
cas_StatusReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 02 06 40 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00

- No.: 3618
- Timestamp: 10:52:50:501_1
- RFN: 5043
- Chip: 19200
- Event: Start Timer
- Source: tc_7_2_3_19:lt_MonitorUplink LINE 1
- Message Structure:
no details available
- Constraint:
t_WaitMS (4000 Ms)
- BinaryMessage:

- No.: 3622
- Timestamp: 10:52:54:499_0
- RFN: 5443
- Chip: 12288
- Event: Timeout
- Source: tc_7_2_3_19:lt_MonitorUplink LINE 3
- Message Structure:
no details available
- Constraint:
t_WaitMS
- BinaryMessage:

- No.: 3625
- Timestamp: 10:52:54:503_0
- RFN: 5443
- Chip: 25088
- Event: Start Timer
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 11
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 3632
- Timestamp: 10:52:54:522_0
- RFN: 5445
- Chip: 20992
- Event: Timeout
- Source: tc_7_2_3_19:lt_TxAndRx LINE 6
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 3655
- Timestamp: 10:52:54:570_0
- RFN: 5450
- Chip: 15616
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000001'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000010'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000110'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001000'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001010'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'ABEECE4B0B813FD337873F'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 09 05 09 0d 11 14 ab ee ce 4b 0b 81 3f d3 37 87 3f

- No.: 3664
- Timestamp: 10:52:54:584_1
- RFN: 5451
- Chip: 31488
- Event: Start Timer
- Source: tc_7_2_3_19:lt_TxAndRx LINE 10
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 3665
- Timestamp: 10:52:54:584_2
- RFN: 5451
- Chip: 32512
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3670
- Timestamp: 10:52:54:594_0
- RFN: 5452
- Chip: 29952
- Event: Timeout
- Source: tc_7_2_3_19:lt_TxAndRx LINE 6
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 3672
- Timestamp: 10:52:54:597_0
- RFN: 5453
- Chip: 3072
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3677
- Timestamp: 10:52:54:753_0
- RFN: 5468
- Chip: 28928
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001100100'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111011100000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101010111110111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '000010001010101'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'EE08ABEE08'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 20 08 ab ee 08 ab ee 08 ab ee 08 ab ee 08 ab ee 08

- No.: 3681
- Timestamp: 10:52:54:759_1
- RFN: 5469
- Chip: 13056
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3686
- Timestamp: 10:52:54:774_0
- RFN: 5470
- Chip: 29952
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001100101'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '000010001010101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111011100000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101010111110111'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '08ABEE08AB'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 28 ab ee 08 ab ee 08 ab ee 08 ab ee 08 ab ee 08 ab

- No.: 3690
- Timestamp: 10:52:54:780_2
- RFN: 5471
- Chip: 14592
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3695
- Timestamp: 10:52:54:794_0
- RFN: 5472
- Chip: 30976
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001100110'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101010111110111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '000010001010101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111011100000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = 'ABEE08ABEE'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 30 ee 08 ab ee 08 ab ee 08 ab ee 08 ab ee 08 ab ee

- No.: 3699
- Timestamp: 10:52:54:800_3
- RFN: 5473
- Chip: 15616
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3704
- Timestamp: 10:52:54:814_0
- RFN: 5474
- Chip: 31744
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001100111'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111011100000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101010111110111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '000010001010101'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'EE08ABEE08'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 38 08 ab ee 08 ab ee 08 ab ee 08 ab ee 08 ab ee 08

- No.: 3708
- Timestamp: 10:52:54:820_3
- RFN: 5475
- Chip: 15872
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3713
- Timestamp: 10:52:54:835_0
- RFN: 5476
- Chip: 32768
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001101000'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '000010001010101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111011100000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101010111110111'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '08ABEE08AB'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 40 ab ee 08 ab ee 08 ab ee 08 ab ee 08 ab ee 08 ab

- No.: 3717
- Timestamp: 10:52:54:840_3
- RFN: 5477
- Chip: 16896
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3722
- Timestamp: 10:52:54:855_0
- RFN: 5478
- Chip: 34048
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001101001'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101010111110111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '000010001010101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111011100000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = 'ABEE08ABEE'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 48 ee 08 ab ee 08 ab ee 08 ab ee 08 ab ee 08 ab ee

- No.: 3726
- Timestamp: 10:52:54:861_1
- RFN: 5479
- Chip: 18432
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3731
- Timestamp: 10:52:54:875_0
- RFN: 5480
- Chip: 34560
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001101010'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111011100000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101010111110111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '000010001010101'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'EE08ABEE08'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 50 08 ab ee 08 ab ee 08 ab ee 08 ab ee 08 ab ee 08

- No.: 3735
- Timestamp: 10:52:54:881_1
- RFN: 5481
- Chip: 19200
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3740
- Timestamp: 10:52:54:895_0
- RFN: 5482
- Chip: 35328
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001101011'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '000010001010101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111011100000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101010111110111'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '08ABEE08AB'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 58 ab ee 08 ab ee 08 ab ee 08 ab ee 08 ab ee 08 ab

- No.: 3744
- Timestamp: 10:52:54:901_2
- RFN: 5483
- Chip: 19712
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3747
- Timestamp: 10:52:54:913_0
- RFN: 5484
- Chip: 28160
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001101100'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101010111110111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '000010001010101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111011100000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = 'ABEE08ABEE'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 60 ee 08 ab ee 08 ab ee 08 ab ee 08 ab ee 08 ab ee

- No.: 3751
- Timestamp: 10:52:54:919_2
- RFN: 5485
- Chip: 12288
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3756
- Timestamp: 10:52:54:933_0
- RFN: 5486
- Chip: 28672
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001101101'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111011100000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101010111110111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '000010001010101'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'EE08ABEE08'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 68 08 ab ee 08 ab ee 08 ab ee 08 ab ee 08 ab ee 08

- No.: 3760
- Timestamp: 10:52:54:939_2
- RFN: 5487
- Chip: 13056
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3765
- Timestamp: 10:52:54:954_0
- RFN: 5488
- Chip: 30464
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001101110'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '000010001010101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111011100000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101010111110111'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '08ABEE08AB'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 70 ab ee 08 ab ee 08 ab ee 08 ab ee 08 ab ee 08 ab

- No.: 3769
- Timestamp: 10:52:54:960_0
- RFN: 5489
- Chip: 16128
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3774
- Timestamp: 10:52:54:975_0
- RFN: 5490
- Chip: 35328
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001101111'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101010111110111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '000010001010101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111011100000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = 'ABEE08ABEE'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 78 ee 08 ab ee 08 ab ee 08 ab ee 08 ab ee 08 ab ee

- No.: 3778
- Timestamp: 10:52:54:981_1
- RFN: 5491
- Chip: 19968
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3781
- Timestamp: 10:52:54:993_0
- RFN: 5492
- Chip: 27136
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001110000'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111011100000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101010111110111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '000010001010101'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'EE08ABEE08'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 80 08 ab ee 08 ab ee 08 ab ee 08 ab ee 08 ab ee 08

- No.: 3785
- Timestamp: 10:52:54:999_0
- RFN: 5493
- Chip: 11520
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3790
- Timestamp: 10:52:55:013_0
- RFN: 5494
- Chip: 27904
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001110001'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '000010001010101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111011100000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101010111110111'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '08ABEE08AB'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 88 ab ee 08 ab ee 08 ab ee 08 ab ee 08 ab ee 08 ab

- No.: 3794
- Timestamp: 10:52:55:019_1
- RFN: 5495
- Chip: 12288
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3799
- Timestamp: 10:52:55:033_0
- RFN: 5496
- Chip: 30208
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001110010'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101010111110111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '000010001010101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111011100000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = 'ABEE08ABEE'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 90 ee 08 ab ee 08 ab ee 08 ab ee 08 ab ee 08 ab ee

- No.: 3803
- Timestamp: 10:52:55:039_3
- RFN: 5497
- Chip: 14592
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3808
- Timestamp: 10:52:55:054_0
- RFN: 5498
- Chip: 32256
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001110011'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111011100000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101010111110111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '000010001010101'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'EE08ABEE08'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 98 08 ab ee 08 ab ee 08 ab ee 08 ab ee 08 ab ee 08

- No.: 3812
- Timestamp: 10:52:55:060_1
- RFN: 5499
- Chip: 16896
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3817
- Timestamp: 10:52:55:075_0
- RFN: 5500
- Chip: 34048
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001110100'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '000010001010101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111011100000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101010111110111'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '08ABEE08AB'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 a0 ab ee 08 ab ee 08 ab ee 08 ab ee 08 ab ee 08 ab

- No.: 3821
- Timestamp: 10:52:55:081_2
- RFN: 5501
- Chip: 18432
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3826
- Timestamp: 10:52:55:096_0
- RFN: 5502
- Chip: 37632
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001110101'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101010111110111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '000010001010101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111011100000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = 'ABEE08ABEE'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 a8 ee 08 ab ee 08 ab ee 08 ab ee 08 ab ee 08 ab ee

- No.: 3830
- Timestamp: 10:52:55:102_2
- RFN: 5503
- Chip: 22272
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3835
- Timestamp: 10:52:55:116_0
- RFN: 5505
- Chip: 512
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001110110'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111011100000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101010111110111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '000010001010101'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'EE08ABEE08'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 b0 08 ab ee 08 ab ee 08 ab ee 08 ab ee 08 ab ee 08

- No.: 3839
- Timestamp: 10:52:55:124_2
- RFN: 5505
- Chip: 32000
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3842
- Timestamp: 10:52:55:134_0
- RFN: 5506
- Chip: 31488
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001110111'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1110111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1010101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '111011100000100'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '101010111110111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '000010001010101'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'EE08ABEE08'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 b9 1e ab ee 08 ab ee 08 ab ee 08 ab ee 08 ab ee 08

- No.: 3846
- Timestamp: 10:52:55:140_3
- RFN: 5507
- Chip: 15616
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3851
- Timestamp: 10:52:55:155_0
- RFN: 5508
- Chip: 33280
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001111000'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0100101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0100101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010010111100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010010111100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010010111100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '4BCE4BCE4B'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 c0 ce 4b ce 4b ce 4b ce 4b ce 4b ce 4b ce 4b ce 4b

- No.: 3855
- Timestamp: 10:52:55:161_0
- RFN: 5509
- Chip: 17408
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3860
- Timestamp: 10:52:55:175_0
- RFN: 5510
- Chip: 34304
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001111001'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0100101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0100101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010010111100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010010111100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010010111100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '4BCE4BCE4B'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 c8 ce 4b ce 4b ce 4b ce 4b ce 4b ce 4b ce 4b ce 4b

- No.: 3864
- Timestamp: 10:52:55:181_1
- RFN: 5511
- Chip: 18432
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3869
- Timestamp: 10:52:55:195_0
- RFN: 5512
- Chip: 35584
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001111010'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0100101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0100101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010010111100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010010111100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010010111100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '4BCE4BCE4B'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 d0 ce 4b ce 4b ce 4b ce 4b ce 4b ce 4b ce 4b ce 4b

- No.: 3873
- Timestamp: 10:52:55:201_2
- RFN: 5513
- Chip: 19968
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3878
- Timestamp: 10:52:55:216_0
- RFN: 5515
- Chip: 2048
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001111011'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0100101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0100101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010010111100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010010111100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010010111100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '4BCE4BCE4B'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 d8 ce 4b ce 4b ce 4b ce 4b ce 4b ce 4b ce 4b ce 4b

- No.: 3882
- Timestamp: 10:52:55:225_1
- RFN: 5515
- Chip: 34560
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3885
- Timestamp: 10:52:55:235_0
- RFN: 5516
- Chip: 35072
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001111100'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0100101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0100101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010010111100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010010111100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010010111100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '4BCE4BCE4B'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 e0 ce 4b ce 4b ce 4b ce 4b ce 4b ce 4b ce 4b ce 4b

- No.: 3889
- Timestamp: 10:52:55:241_2
- RFN: 5517
- Chip: 20480
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3892
- Timestamp: 10:52:55:253_0
- RFN: 5518
- Chip: 28672
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001111101'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0100101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0100101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010010111100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010010111100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010010111100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '4BCE4BCE4B'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 e8 ce 4b ce 4b ce 4b ce 4b ce 4b ce 4b ce 4b ce 4b

- No.: 3896
- Timestamp: 10:52:55:259_3
- RFN: 5519
- Chip: 13568
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3901
- Timestamp: 10:52:55:276_0
- RFN: 5521
- Chip: 0
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001111110'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0100101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0100101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010010111100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010010111100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010010111100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '4BCE4BCE4B'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 f0 ce 4b ce 4b ce 4b ce 4b ce 4b ce 4b ce 4b ce 4b

- No.: 3905
- Timestamp: 10:52:55:284_1
- RFN: 5521
- Chip: 31744
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3908
- Timestamp: 10:52:55:294_0
- RFN: 5522
- Chip: 31488
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001111111'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0100101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0100101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010010111100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010010111100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010010111100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '4BCE4BCE4B'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 f8 ce 4b ce 4b ce 4b ce 4b ce 4b ce 4b ce 4b ce 4b

- No.: 3912
- Timestamp: 10:52:55:300_1
- RFN: 5523
- Chip: 16128
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3917
- Timestamp: 10:52:55:314_0
- RFN: 5524
- Chip: 33280
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000010000000'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0100101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0100101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010010111100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010010111100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010010111100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '4BCE4BCE4B'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 84 00 ce 4b ce 4b ce 4b ce 4b ce 4b ce 4b ce 4b ce 4b

- No.: 3921
- Timestamp: 10:52:55:320_2
- RFN: 5525
- Chip: 17664
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3926
- Timestamp: 10:52:55:335_0
- RFN: 5526
- Chip: 35328
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000010000001'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0100101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0100101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010010111100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010010111100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010010111100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '4BCE4BCE4B'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 84 08 ce 4b ce 4b ce 4b ce 4b ce 4b ce 4b ce 4b ce 4b

- No.: 3930
- Timestamp: 10:52:55:341_0
- RFN: 5527
- Chip: 19968
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3935
- Timestamp: 10:52:55:356_0
- RFN: 5529
- Chip: 2816
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000010000010'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0100101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0100101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010010111100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010010111100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010010111100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '4BCE4BCE4B'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 84 10 ce 4b ce 4b ce 4b ce 4b ce 4b ce 4b ce 4b ce 4b

- No.: 3939
- Timestamp: 10:52:55:364_3
- RFN: 5529
- Chip: 34560
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3942
- Timestamp: 10:52:55:374_0
- RFN: 5530
- Chip: 33280
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000010000011'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0100101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0100101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010010111100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010010111100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010010111100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '4BCE4BCE4B'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 84 18 ce 4b ce 4b ce 4b ce 4b ce 4b ce 4b ce 4b ce 4b

- No.: 3946
- Timestamp: 10:52:55:380_2
- RFN: 5531
- Chip: 18432
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3951
- Timestamp: 10:52:55:396_0
- RFN: 5532
- Chip: 35584
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000010000100'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0100101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0100101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010010111100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010010111100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010010111100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '4BCE4BCE4B'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 84 20 ce 4b ce 4b ce 4b ce 4b ce 4b ce 4b ce 4b ce 4b

- No.: 3955
- Timestamp: 10:52:55:402_0
- RFN: 5533
- Chip: 20480
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3958
- Timestamp: 10:52:55:414_0
- RFN: 5534
- Chip: 27904
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000010000101'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0100101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0100101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010010111100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010010111100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010010111100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '4BCE4BCE4B'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 84 28 ce 4b ce 4b ce 4b ce 4b ce 4b ce 4b ce 4b ce 4b

- No.: 3962
- Timestamp: 10:52:55:420_0
- RFN: 5535
- Chip: 12800
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3967
- Timestamp: 10:52:55:434_0
- RFN: 5536
- Chip: 30720
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000010000110'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0100101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0100101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010010111100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010010111100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010010111100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '4BCE4BCE4B'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 84 30 ce 4b ce 4b ce 4b ce 4b ce 4b ce 4b ce 4b ce 4b

- No.: 3971
- Timestamp: 10:52:55:440_2
- RFN: 5537
- Chip: 15360
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3976
- Timestamp: 10:52:55:455_0
- RFN: 5538
- Chip: 33024
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000010000111'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0100101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0100101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010010111100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010010111100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010010111100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '4BCE4BCE4B'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 84 38 ce 4b ce 4b ce 4b ce 4b ce 4b ce 4b ce 4b ce 4b

- No.: 3980
- Timestamp: 10:52:55:461_0
- RFN: 5539
- Chip: 17664
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3985
- Timestamp: 10:52:55:475_0
- RFN: 5540
- Chip: 35840
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000010001000'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0100101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0100101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010010111100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010010111100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010010111100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '4BCE4BCE4B'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 84 40 ce 4b ce 4b ce 4b ce 4b ce 4b ce 4b ce 4b ce 4b

- No.: 3989
- Timestamp: 10:52:55:481_3
- RFN: 5541
- Chip: 20480
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3992
- Timestamp: 10:52:55:494_0
- RFN: 5542
- Chip: 30464
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000010001001'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0100101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0100101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010010111100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010010111100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010010111100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '4BCE4BCE4B'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 84 48 ce 4b ce 4b ce 4b ce 4b ce 4b ce 4b ce 4b ce 4b

- No.: 3996
- Timestamp: 10:52:55:500_1
- RFN: 5543
- Chip: 14848
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4001
- Timestamp: 10:52:55:514_0
- RFN: 5544
- Chip: 32768
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000010001010'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0100101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0100101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010010111100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010010111100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '010010111100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . (AM_Data)data[5] = '4BCE4BCE4B'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 84 50 ce 4b ce 4b ce 4b ce 4b ce 4b ce 4b ce 4b ce 4b

- No.: 4005
- Timestamp: 10:52:55:520_3
- RFN: 5545
- Chip: 17152
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4010
- Timestamp: 10:52:55:535_0
- RFN: 5546
- Chip: 35072
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000010001011'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0100101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1100111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0100101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110011100100101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110011100100101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110011100100101'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'CE4BCE4BCE'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 84 59 1e ce 4b ce 4b ce 4b ce 4b ce 4b ce 4b ce 4b ce

- No.: 4014
- Timestamp: 10:52:55:541_1
- RFN: 5547
- Chip: 19200
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4019
- Timestamp: 10:52:55:556_0
- RFN: 5548
- Chip: 37632
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000010001100'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000000'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000000'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100000010000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100000010000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100000010000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = '810B810B81'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 84 60 0b 81 0b 81 0b 81 0b 81 0b 81 0b 81 0b 81 0b 81

- No.: 4023
- Timestamp: 10:52:55:564_0
- RFN: 5549
- Chip: 29952
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4026
- Timestamp: 10:52:55:574_0
- RFN: 5550
- Chip: 30208
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000010001101'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000000'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000000'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100000010000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100000010000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100000010000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = '810B810B81'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 84 68 0b 81 0b 81 0b 81 0b 81 0b 81 0b 81 0b 81 0b 81

- No.: 4030
- Timestamp: 10:52:55:580_0
- RFN: 5551
- Chip: 15104
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4035
- Timestamp: 10:52:55:594_0
- RFN: 5552
- Chip: 32256
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000010001110'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000000'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000000'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100000010000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100000010000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100000010000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = '810B810B81'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 84 70 0b 81 0b 81 0b 81 0b 81 0b 81 0b 81 0b 81 0b 81

- No.: 4039
- Timestamp: 10:52:55:600_1
- RFN: 5553
- Chip: 16128
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4044
- Timestamp: 10:52:55:615_0
- RFN: 5554
- Chip: 34816
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000010001111'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000000'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000000'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100000010000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100000010000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100000010000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = '810B810B81'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 84 78 0b 81 0b 81 0b 81 0b 81 0b 81 0b 81 0b 81 0b 81

- No.: 4048
- Timestamp: 10:52:55:621_0
- RFN: 5555
- Chip: 18944
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4053
- Timestamp: 10:52:55:635_0
- RFN: 5556
- Chip: 35584
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000010010000'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000000'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000000'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100000010000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100000010000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100000010000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = '810B810B81'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 84 80 0b 81 0b 81 0b 81 0b 81 0b 81 0b 81 0b 81 0b 81

- No.: 4057
- Timestamp: 10:52:55:641_1
- RFN: 5557
- Chip: 20224
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4062
- Timestamp: 10:52:55:656_0
- RFN: 5559
- Chip: 2048
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000010010001'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000000'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000000'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100000010000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100000010000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100000010000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = '810B810B81'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 84 88 0b 81 0b 81 0b 81 0b 81 0b 81 0b 81 0b 81 0b 81

- No.: 4066
- Timestamp: 10:52:55:664_3
- RFN: 5559
- Chip: 34048
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4069
- Timestamp: 10:52:55:674_0
- RFN: 5560
- Chip: 33792
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000010010010'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000000'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000000'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100000010000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100000010000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100000010000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = '810B810B81'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 84 90 0b 81 0b 81 0b 81 0b 81 0b 81 0b 81 0b 81 0b 81

- No.: 4073
- Timestamp: 10:52:55:680_2
- RFN: 5561
- Chip: 18176
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4078
- Timestamp: 10:52:55:695_0
- RFN: 5563
- Chip: 512
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000010010011'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000000'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000000'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100000010000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100000010000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100000010000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = '810B810B81'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 84 98 0b 81 0b 81 0b 81 0b 81 0b 81 0b 81 0b 81 0b 81

- No.: 4082
- Timestamp: 10:52:55:705_0
- RFN: 5563
- Chip: 32000
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4085
- Timestamp: 10:52:55:714_0
- RFN: 5564
- Chip: 31488
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000010010100'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000000'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000000'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100000010000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100000010000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100000010000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = '810B810B81'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 84 a0 0b 81 0b 81 0b 81 0b 81 0b 81 0b 81 0b 81 0b 81

- No.: 4089
- Timestamp: 10:52:55:720_2
- RFN: 5565
- Chip: 15104
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4094
- Timestamp: 10:52:55:735_0
- RFN: 5566
- Chip: 33280
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000010010101'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000000'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000000'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100000010000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100000010000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100000010000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = '810B810B81'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 84 a8 0b 81 0b 81 0b 81 0b 81 0b 81 0b 81 0b 81 0b 81

- No.: 4098
- Timestamp: 10:52:55:741_0
- RFN: 5567
- Chip: 16896
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4103
- Timestamp: 10:52:55:755_0
- RFN: 5568
- Chip: 34816
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000010010110'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000000'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000000'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100000010000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100000010000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100000010000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = '810B810B81'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 84 b0 0b 81 0b 81 0b 81 0b 81 0b 81 0b 81 0b 81 0b 81

- No.: 4107
- Timestamp: 10:52:55:761_2
- RFN: 5569
- Chip: 18944
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4112
- Timestamp: 10:52:55:775_0
- RFN: 5570
- Chip: 35584
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000010010111'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000000'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000000'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100000010000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100000010000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100000010000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = '810B810B81'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 84 b8 0b 81 0b 81 0b 81 0b 81 0b 81 0b 81 0b 81 0b 81

- No.: 4116
- Timestamp: 10:52:55:781_2
- RFN: 5571
- Chip: 19200
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4121
- Timestamp: 10:52:55:795_0
- RFN: 5572
- Chip: 36352
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000010011000'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000000'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000000'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100000010000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100000010000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100000010000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = '810B810B81'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 84 c0 0b 81 0b 81 0b 81 0b 81 0b 81 0b 81 0b 81 0b 81

- No.: 4125
- Timestamp: 10:52:55:801_3
- RFN: 5573
- Chip: 20224
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4128
- Timestamp: 10:52:55:813_0
- RFN: 5574
- Chip: 28416
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000010011001'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000000'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000000'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100000010000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100000010000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100000010000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = '810B810B81'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 84 c8 0b 81 0b 81 0b 81 0b 81 0b 81 0b 81 0b 81 0b 81

- No.: 4132
- Timestamp: 10:52:55:819_2
- RFN: 5575
- Chip: 12032
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4137
- Timestamp: 10:52:55:834_0
- RFN: 5576
- Chip: 29696
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000010011010'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000000'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000000'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100000010000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100000010000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100000010000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = '810B810B81'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 84 d0 0b 81 0b 81 0b 81 0b 81 0b 81 0b 81 0b 81 0b 81

- No.: 4141
- Timestamp: 10:52:55:840_1
- RFN: 5577
- Chip: 15616
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4146
- Timestamp: 10:52:55:855_0
- RFN: 5578
- Chip: 33536
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000010011011'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000000'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000000'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100000010000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100000010000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100000010000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = '810B810B81'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 84 d8 0b 81 0b 81 0b 81 0b 81 0b 81 0b 81 0b 81 0b 81

- No.: 4150
- Timestamp: 10:52:55:860_3
- RFN: 5579
- Chip: 17408
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4155
- Timestamp: 10:52:55:875_0
- RFN: 5580
- Chip: 34560
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000010011100'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000000'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000000'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100000010000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100000010000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100000010000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = '810B810B81'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 84 e0 0b 81 0b 81 0b 81 0b 81 0b 81 0b 81 0b 81 0b 81

- No.: 4159
- Timestamp: 10:52:55:881_0
- RFN: 5581
- Chip: 18688
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4164
- Timestamp: 10:52:55:895_0
- RFN: 5582
- Chip: 35328
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000010011101'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000000'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000000'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100000010000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100000010000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100000010000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = '810B810B81'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 84 e8 0b 81 0b 81 0b 81 0b 81 0b 81 0b 81 0b 81 0b 81

- No.: 4168
- Timestamp: 10:52:55:901_2
- RFN: 5583
- Chip: 20480
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4171
- Timestamp: 10:52:55:914_0
- RFN: 5584
- Chip: 30464
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000010011110'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000000'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000000'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100000010000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100000010000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100000010000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = '810B810B81'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 84 f0 0b 81 0b 81 0b 81 0b 81 0b 81 0b 81 0b 81 0b 81

- No.: 4175
- Timestamp: 10:52:55:919_3
- RFN: 5585
- Chip: 14336
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4180
- Timestamp: 10:52:55:934_0
- RFN: 5586
- Chip: 32000
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000010011111'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000000'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0000101'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000000'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '000010111000000'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '000010111000000'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '000010111000000'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = '0B810B810B'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 84 f9 1e 0b 81 0b 81 0b 81 0b 81 0b 81 0b 81 0b 81 0b

- No.: 4184
- Timestamp: 10:52:55:940_1
- RFN: 5587
- Chip: 16640
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4189
- Timestamp: 10:52:55:954_0
- RFN: 5588
- Chip: 34048
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000010100000'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1101001'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1101001'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110100110011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110100110011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110100110011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'D33FD33FD3'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 85 00 3f d3 3f d3 3f d3 3f d3 3f d3 3f d3 3f d3 3f d3

- No.: 4193
- Timestamp: 10:52:55:960_2
- RFN: 5589
- Chip: 17920
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4198
- Timestamp: 10:52:55:975_0
- RFN: 5590
- Chip: 36096
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000010100001'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1101001'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1101001'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110100110011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110100110011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110100110011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'D33FD33FD3'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 85 08 3f d3 3f d3 3f d3 3f d3 3f d3 3f d3 3f d3 3f d3

- No.: 4202
- Timestamp: 10:52:55:981_0
- RFN: 5591
- Chip: 19712
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4205
- Timestamp: 10:52:55:993_0
- RFN: 5592
- Chip: 27648
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000010100010'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1101001'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1101001'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110100110011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110100110011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110100110011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'D33FD33FD3'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 85 10 3f d3 3f d3 3f d3 3f d3 3f d3 3f d3 3f d3 3f d3

- No.: 4209
- Timestamp: 10:52:55:998_3
- RFN: 5593
- Chip: 11008
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4214
- Timestamp: 10:52:56:013_0
- RFN: 5594
- Chip: 29952
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000010100011'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1101001'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1101001'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110100110011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110100110011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110100110011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'D33FD33FD3'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 85 18 3f d3 3f d3 3f d3 3f d3 3f d3 3f d3 3f d3 3f d3

- No.: 4218
- Timestamp: 10:52:56:020_2
- RFN: 5595
- Chip: 14592
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4223
- Timestamp: 10:52:56:036_0
- RFN: 5596
- Chip: 37632
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000010100100'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1101001'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1101001'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110100110011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110100110011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110100110011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'D33FD33FD3'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 85 20 3f d3 3f d3 3f d3 3f d3 3f d3 3f d3 3f d3 3f d3

- No.: 4227
- Timestamp: 10:52:56:043_0
- RFN: 5597
- Chip: 24832
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4232
- Timestamp: 10:52:56:057_0
- RFN: 5599
- Chip: 2048
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000010100101'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1101001'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1101001'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110100110011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110100110011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110100110011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'D33FD33FD3'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 85 28 3f d3 3f d3 3f d3 3f d3 3f d3 3f d3 3f d3 3f d3

- No.: 4236
- Timestamp: 10:52:56:065_1
- RFN: 5599
- Chip: 33280
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4239
- Timestamp: 10:52:56:075_0
- RFN: 5600
- Chip: 32512
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000010100110'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1101001'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1101001'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110100110011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110100110011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110100110011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'D33FD33FD3'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 85 30 3f d3 3f d3 3f d3 3f d3 3f d3 3f d3 3f d3 3f d3

- No.: 4243
- Timestamp: 10:52:56:080_3
- RFN: 5601
- Chip: 16128
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4248
- Timestamp: 10:52:56:095_0
- RFN: 5602
- Chip: 34048
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000010100111'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1101001'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1101001'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110100110011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110100110011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110100110011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'D33FD33FD3'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 85 38 3f d3 3f d3 3f d3 3f d3 3f d3 3f d3 3f d3 3f d3

- No.: 4252
- Timestamp: 10:52:56:101_2
- RFN: 5603
- Chip: 18944
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4257
- Timestamp: 10:52:56:116_0
- RFN: 5605
- Chip: 1792
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000010101000'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1101001'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1101001'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110100110011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110100110011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110100110011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'D33FD33FD3'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 85 40 3f d3 3f d3 3f d3 3f d3 3f d3 3f d3 3f d3 3f d3

- No.: 4261
- Timestamp: 10:52:56:123_3
- RFN: 5605
- Chip: 27904
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4266
- Timestamp: 10:52:56:137_0
- RFN: 5607
- Chip: 3328
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000010101001'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1101001'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1101001'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110100110011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110100110011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110100110011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'D33FD33FD3'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 85 48 3f d3 3f d3 3f d3 3f d3 3f d3 3f d3 3f d3 3f d3

- No.: 4270
- Timestamp: 10:52:56:145_1
- RFN: 5607
- Chip: 34304
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4273
- Timestamp: 10:52:56:155_0
- RFN: 5608
- Chip: 33792
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000010101010'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1101001'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1101001'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110100110011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110100110011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110100110011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'D33FD33FD3'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 85 50 3f d3 3f d3 3f d3 3f d3 3f d3 3f d3 3f d3 3f d3

- No.: 4277
- Timestamp: 10:52:56:160_3
- RFN: 5609
- Chip: 17152
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4282
- Timestamp: 10:52:56:175_0
- RFN: 5610
- Chip: 35584
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000010101011'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1101001'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1101001'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110100110011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110100110011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110100110011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'D33FD33FD3'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 85 58 3f d3 3f d3 3f d3 3f d3 3f d3 3f d3 3f d3 3f d3

- No.: 4286
- Timestamp: 10:52:56:181_2
- RFN: 5611
- Chip: 20480
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4289
- Timestamp: 10:52:56:194_0
- RFN: 5612
- Chip: 30208
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000010101100'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1101001'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1101001'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110100110011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110100110011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110100110011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'D33FD33FD3'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 85 60 3f d3 3f d3 3f d3 3f d3 3f d3 3f d3 3f d3 3f d3

- No.: 4293
- Timestamp: 10:52:56:200_1
- RFN: 5613
- Chip: 15360
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4298
- Timestamp: 10:52:56:217_0
- RFN: 5615
- Chip: 5376
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000010101101'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1101001'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1101001'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110100110011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110100110011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110100110011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'D33FD33FD3'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 85 68 3f d3 3f d3 3f d3 3f d3 3f d3 3f d3 3f d3 3f d3

- No.: 4302
- Timestamp: 10:52:56:225_2
- RFN: 5615
- Chip: 36864
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4305
- Timestamp: 10:52:56:235_0
- RFN: 5616
- Chip: 36096
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000010101110'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1101001'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1101001'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110100110011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110100110011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110100110011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'D33FD33FD3'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 85 70 3f d3 3f d3 3f d3 3f d3 3f d3 3f d3 3f d3 3f d3

- No.: 4309
- Timestamp: 10:52:56:241_1
- RFN: 5617
- Chip: 20224
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4314
- Timestamp: 10:52:56:258_0
- RFN: 5619
- Chip: 7680
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000010101111'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1101001'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1101001'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110100110011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110100110011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110100110011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'D33FD33FD3'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 85 78 3f d3 3f d3 3f d3 3f d3 3f d3 3f d3 3f d3 3f d3

- No.: 4318
- Timestamp: 10:52:56:266_0
- RFN: 5619
- Chip: 38144
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4321
- Timestamp: 10:52:56:275_0
- RFN: 5620
- Chip: 37120
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000010110000'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1101001'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1101001'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110100110011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110100110011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110100110011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'D33FD33FD3'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 85 80 3f d3 3f d3 3f d3 3f d3 3f d3 3f d3 3f d3 3f d3

- No.: 4325
- Timestamp: 10:52:56:281_1
- RFN: 5621
- Chip: 20736
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4330
- Timestamp: 10:52:56:295_0
- RFN: 5622
- Chip: 37632
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000010110001'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1101001'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1101001'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110100110011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110100110011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110100110011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'D33FD33FD3'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 85 88 3f d3 3f d3 3f d3 3f d3 3f d3 3f d3 3f d3 3f d3

- No.: 4334
- Timestamp: 10:52:56:303_0
- RFN: 5623
- Chip: 29952
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4337
- Timestamp: 10:52:56:313_0
- RFN: 5624
- Chip: 29952
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000010110010'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1101001'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1101001'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110100110011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110100110011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '110100110011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = 'D33FD33FD3'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 85 90 3f d3 3f d3 3f d3 3f d3 3f d3 3f d3 3f d3 3f d3

- No.: 4341
- Timestamp: 10:52:56:319_1
- RFN: 5625
- Chip: 13568
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4346
- Timestamp: 10:52:56:334_0
- RFN: 5626
- Chip: 30976
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000010110011'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1101001'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011111'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1101001'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '001111111101001'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '001111111101001'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '001111111101001'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = '3FD33FD33F'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 85 99 1e 3f d3 3f d3 3f d3 3f d3 3f d3 3f d3 3f d3 3f

- No.: 4350
- Timestamp: 10:52:56:340_3
- RFN: 5627
- Chip: 15360
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4355
- Timestamp: 10:52:56:356_0
- RFN: 5628
- Chip: 36864
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000010110100'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100001110011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100001110011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100001110011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = '8737873787'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 85 a0 37 87 37 87 37 87 37 87 37 87 37 87 37 87 37 87

- No.: 4359
- Timestamp: 10:52:56:363_0
- RFN: 5629
- Chip: 24320
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4364
- Timestamp: 10:52:56:376_0
- RFN: 5631
- Chip: 256
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000010110101'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100001110011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100001110011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100001110011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = '8737873787'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 85 a8 37 87 37 87 37 87 37 87 37 87 37 87 37 87 37 87

- No.: 4368
- Timestamp: 10:52:56:384_1
- RFN: 5631
- Chip: 30976
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4371
- Timestamp: 10:52:56:394_0
- RFN: 5632
- Chip: 29952
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000010110110'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100001110011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100001110011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100001110011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = '8737873787'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 85 b0 37 87 37 87 37 87 37 87 37 87 37 87 37 87 37 87

- No.: 4375
- Timestamp: 10:52:56:400_0
- RFN: 5633
- Chip: 14080
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4380
- Timestamp: 10:52:56:414_0
- RFN: 5634
- Chip: 32256
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000010110111'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100001110011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100001110011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100001110011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = '8737873787'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 85 b8 37 87 37 87 37 87 37 87 37 87 37 87 37 87 37 87

- No.: 4384
- Timestamp: 10:52:56:421_0
- RFN: 5635
- Chip: 17152
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4389
- Timestamp: 10:52:56:436_0
- RFN: 5637
- Chip: 256
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000010111000'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100001110011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100001110011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100001110011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = '8737873787'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 85 c0 37 87 37 87 37 87 37 87 37 87 37 87 37 87 37 87

- No.: 4393
- Timestamp: 10:52:56:442_1
- RFN: 5637
- Chip: 24576
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4396
- Timestamp: 10:52:56:454_0
- RFN: 5638
- Chip: 30720
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000010111001'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100001110011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100001110011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100001110011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = '8737873787'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 85 c8 37 87 37 87 37 87 37 87 37 87 37 87 37 87 37 87

- No.: 4400
- Timestamp: 10:52:56:460_1
- RFN: 5639
- Chip: 14848
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4405
- Timestamp: 10:52:56:474_0
- RFN: 5640
- Chip: 32768
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000010111010'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100001110011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100001110011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100001110011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = '8737873787'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 85 d4 37 87 37 87 37 87 37 87 37 87 37 87 37 87 37 87

- No.: 4412
- Timestamp: 10:52:56:491_1
- RFN: 5642
- Chip: 19712
- Event: Read Timer
- Source: tc_7_2_3_19:lt_CheckTimeDiff LINE 1
- Message Structure:
no details available
- Constraint:
t_Dly (6010 ÌÌÌÌÌÌÌÌ)
- BinaryMessage:

- No.: 4414
- Timestamp: 10:52:56:494_1
- RFN: 5642
- Chip: 32000
- Event: Cancel Timer
- Source: tc_7_2_3_19:lt_CheckTimeDiff LINE 2
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 4418
- Timestamp: 10:52:56:498_0
- RFN: 5643
- Chip: 6912
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4421
- Timestamp: 10:52:56:509_0
- RFN: 5644
- Chip: 11520
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000010111011'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100001110011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100001110011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100001110011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = '8737873787'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 85 d8 37 87 37 87 37 87 37 87 37 87 37 87 37 87 37 87

- No.: 4425
- Timestamp: 10:52:56:516_2
- RFN: 5645
- Chip: 1536
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4428
- Timestamp: 10:52:56:528_0
- RFN: 5646
- Chip: 8704
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000010111100'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100001110011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100001110011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100001110011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = '8737873787'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 85 e0 37 87 37 87 37 87 37 87 37 87 37 87 37 87 37 87

- No.: 4432
- Timestamp: 10:52:56:534_3
- RFN: 5646
- Chip: 33536
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4435
- Timestamp: 10:52:56:546_0
- RFN: 5647
- Chip: 38144
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000010111101'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100001110011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100001110011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100001110011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = '8737873787'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 85 e8 37 87 37 87 37 87 37 87 37 87 37 87 37 87 37 87

- No.: 4439
- Timestamp: 10:52:56:551_3
- RFN: 5648
- Chip: 21760
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4444
- Timestamp: 10:52:56:566_0
- RFN: 5650
- Chip: 3072
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000010111110'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100001110011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100001110011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100001110011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = '8737873787'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 85 f0 37 87 37 87 37 87 37 87 37 87 37 87 37 87 37 87

- No.: 4448
- Timestamp: 10:52:56:573_3
- RFN: 5650
- Chip: 29184
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4451
- Timestamp: 10:52:56:585_0
- RFN: 5651
- Chip: 37120
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000010111111'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100001110011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100001110011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100001110011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = '8737873787'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 85 f8 37 87 37 87 37 87 37 87 37 87 37 87 37 87 37 87

- No.: 4455
- Timestamp: 10:52:56:591_3
- RFN: 5652
- Chip: 22784
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4458
- Timestamp: 10:52:56:601_0
- RFN: 5653
- Chip: 19968
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000011000000'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100001110011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100001110011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100001110011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = '8737873787'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 86 00 37 87 37 87 37 87 37 87 37 87 37 87 37 87 37 87

- No.: 4462
- Timestamp: 10:52:56:609_2
- RFN: 5654
- Chip: 14848
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4465
- Timestamp: 10:52:56:619_0
- RFN: 5655
- Chip: 14592
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000011000001'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100001110011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100001110011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100001110011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = '8737873787'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 86 08 37 87 37 87 37 87 37 87 37 87 37 87 37 87 37 87

- No.: 4469
- Timestamp: 10:52:56:628_1
- RFN: 5656
- Chip: 9472
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4472
- Timestamp: 10:52:56:637_0
- RFN: 5657
- Chip: 6400
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000011000010'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100001110011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100001110011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100001110011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = '8737873787'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 86 10 37 87 37 87 37 87 37 87 37 87 37 87 37 87 37 87

- No.: 4476
- Timestamp: 10:52:56:645_3
- RFN: 5657
- Chip: 34560
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4481
- Timestamp: 10:52:56:658_0
- RFN: 5659
- Chip: 8192
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000011000011'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100001110011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100001110011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100001110011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = '8737873787'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 86 18 37 87 37 87 37 87 37 87 37 87 37 87 37 87 37 87

- No.: 4485
- Timestamp: 10:52:56:667_0
- RFN: 5660
- Chip: 1024
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4488
- Timestamp: 10:52:56:676_0
- RFN: 5660
- Chip: 38144
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000011000100'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100001110011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100001110011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100001110011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = '8737873787'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 86 20 37 87 37 87 37 87 37 87 37 87 37 87 37 87 37 87

- No.: 4492
- Timestamp: 10:52:56:684_1
- RFN: 5661
- Chip: 29952
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4497
- Timestamp: 10:52:56:699_0
- RFN: 5663
- Chip: 9728
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000011000101'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100001110011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100001110011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100001110011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = '8737873787'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 86 28 37 87 37 87 37 87 37 87 37 87 37 87 37 87 37 87

- No.: 4501
- Timestamp: 10:52:56:707_2
- RFN: 5664
- Chip: 3072
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4504
- Timestamp: 10:52:56:717_0
- RFN: 5665
- Chip: 2304
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000011000110'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100001110011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100001110011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '100001110011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = '8737873787'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 86 30 37 87 37 87 37 87 37 87 37 87 37 87 37 87 37 87

- No.: 4508
- Timestamp: 10:52:56:723_1
- RFN: 5665
- Chip: 26880
- Event: Repeat
- Source: tc_7_2_3_19:lt_TimerPollPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4511
- Timestamp: 10:52:56:734_0
- RFN: 5666
- Chip: 32256
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000011000111'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '001101111000011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '001101111000011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '001101111000011'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = '3787378737'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 86 39 1e 37 87 37 87 37 87 37 87 37 87 37 87 37 87 37

- No.: 4522
- Timestamp: 10:52:58:473_0
- RFN: 5840
- Chip: 28672
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_19:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000011000111'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0011011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '1000011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '001101111000011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '001101111000011'B
. . . . (ExtBit)extBit[1] = '1'B
. . . LenInd15AndE_Bit
. . . . (LenInd15)lenInd[15] = '001101111000011'B
. . . . (ExtBit)extBit[1] = '1'B
. . (AM_Data)data[5] = '3787378737'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 86 3d 1e 37 87 37 87 37 87 37 87 37 87 37 87 37 87 37

- No.: 4530
- Timestamp: 10:52:58:487_2
- RFN: 5842
- Chip: 6400
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: tc_7_2_3_19:lt_CheckNumPolls LINE 1
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4531
- Timestamp: 10:52:58:493_0
- RFN: 5842
- Chip: 30720
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: tc_7_2_3_19:lt_CheckNumPolls LINE 2
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. STATUS_PDU
. . (DC_Field)dC_Field[1] = '0'B
. . (CtrlPDU_Type)type[3] = '000'B
. . SuperFields
. . . SUFI_WindowSize
. . . SUFI_List
. . . SUFI_RList
. . . SUFI_Bitmap
. . . SUFI_MRW
. . . SUFI_MRW_ACK
. . . SUFI_NoMore
. . . SUFI_Ack
. . . . (SUFI_Type)type[4] = '0010'B
. . . . (AM_SeqNum)lsn[12] = '000011001000'B
. . (HexStringType)superFieldsAndPadRx[-1] = -
. . (Padding)paddingTx[-1] = '0000000000000000000000000000000'H
- Constraint:
cas_StatusReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 02 0c 80 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00

- No.: 4537
- Timestamp: 10:52:58:506_0
- RFN: 5844
- Chip: 1024
- Event: Send
- PCO: Dc
- Message: RRC_DataReq
- Source: ts_TC_OpenUE_TestLoop LINE 6
- Message Structure:
RRC_DataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[-1] = -
. (SapId)sapId[1] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. OPENUETESTLOOP
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)tCProtocolDiscriminator[4] = '1111'B
. . (MsgType)msgType[8] = '01000010'B
- Constraint:
ca_PS_DataReq
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 0f 42

- No.: 4538
- Timestamp: 10:52:58:507_0
- RFN: 5844
- Chip: 4608
- Event: Start Timer
- Source: ts_TC_OpenUE_TestLoop LINE 6
- Message Structure:
no details available
- Constraint:
t_Dly (5000 Ms)
- BinaryMessage:

- No.: 4542
- Timestamp: 10:52:58:809_0
- RFN: 5874
- Chip: 12544
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_TC_OpenUE_TestLoop LINE 7
- Message Structure:
RRC_DataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. (START_Value)start[0] = -
. OPENUETESTLOOPCOMPLETE
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)tCProtocolDiscriminator[4] = '1111'B
. . (MsgType)msgType[8] = '01000011'B
- Constraint:
car_PS_UplinkDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 0f 43

- No.: 4543
- Timestamp: 10:52:58:810_0
- RFN: 5874
- Chip: 15872
- Event: Cancel Timer
- Source: ts_TC_OpenUE_TestLoop LINE 7
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 4544
- Timestamp: 10:52:58:810_1
- RFN: 5874
- Chip: 16896
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_TC_OpenUE_TestLoop LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4556
- Timestamp: 10:52:58:818_0
- RFN: 5875
- Chip: 9728
- Event: Send
- PCO: Dc
- Message: RRC_DataReq
- Source: ts_TC_DeactivateRB_TestMode LINE 6
- Message Structure:
RRC_DataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[-1] = -
. (SapId)sapId[1] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. DEACTIVATERBTESTMODE
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)tCProtocolDiscriminator[4] = '1111'B
. . (MsgType)msgType[8] = '01000110'B
- Constraint:
ca_PS_DataReq
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 0f 46

- No.: 4557
- Timestamp: 10:52:58:819_0
- RFN: 5875
- Chip: 14080
- Event: Start Timer
- Source: ts_TC_DeactivateRB_TestMode LINE 6
- Message Structure:
no details available
- Constraint:
t_Dly (5000 Ms)
- BinaryMessage:

- No.: 4561
- Timestamp: 10:52:59:127_0
- RFN: 5906
- Chip: 4608
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_TC_DeactivateRB_TestMode LINE 7
- Message Structure:
RRC_DataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. (START_Value)start[0] = -
. DEACTIVATERBTESTMODECOMPLETE
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)tCProtocolDiscriminator[4] = '1111'B
. . (MsgType)msgType[8] = '01000111'B
- Constraint:
car_PS_UplinkDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 0f 47

- No.: 4562
- Timestamp: 10:52:59:128_0
- RFN: 5906
- Chip: 8448
- Event: Cancel Timer
- Source: ts_TC_DeactivateRB_TestMode LINE 7
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 4563
- Timestamp: 10:52:59:128_1
- RFN: 5906
- Chip: 9216
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_TC_DeactivateRB_TestMode LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4575
- Timestamp: 10:52:59:136_0
- RFN: 5907
- Chip: 768
- Event: Send
- PCO: UM
- Message: RLC_UM_DATA_REQ
- Source: po_ConnectionAndSS_Rel:lt_Send_RRC_ConnectionRelease LINE 8
- Message Structure:
RLC_UM_DATA_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. uM_message
. . DL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00000000000000000000000000000000"
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . DL_DCCH_MessageType
. . . . RRCConnectionRelease
. . . . . r3
. . . . . . RRCConnectionRelease_r3_IEs
. . . . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . . . (IntegerType)n_308 = 1
. . . . . . . (ReleaseCause)releaseCause = 0
. . . . . . . Rplmn_Information
. . . . . . laterNonCriticalExtensions
. (BooleanType)specialLI = FALSE
- Constraint:
cas_RRC_ConnRelDCCH
- BinaryMessage:
30 10 02 01 ff 02 01 01 80 00 00 00 03 c8 00 01 01 00

- No.: 4579
- Timestamp: 10:52:59:368_0
- RFN: 5930
- Chip: 9472
- Event: Receive
- PCO: UM
- Message: RLC_UM_DATA_IND
- Source: po_ConnectionAndSS_Rel:lt_Send_RRC_ConnectionRelease LINE 9
- Message Structure:
RLC_UM_DATA_IND
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. IntegrityResult
. uM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "10110011101011111111101100111000"
. . . . (IntegerType)rrc_MessageSequenceNumber = 1
. . . UL_DCCH_MessageType
. . . . RRCConnectionReleaseComplete
. . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . FailureCauseWithProtErr
. . . . . laterNonCriticalExtensions
. . . . . . (BitStringType)rrcConnectionReleaseComplete_r3_add_ext = 0
. . . . . . nonCriticalExtensions
- Constraint:
car_RRC_ConnRelCmplUM
- BinaryMessage:
30 0c 02 01 ff 02 01 01 d9 d7 fd 9c 0c 40

- No.: 4580
- Timestamp: 10:52:59:369_0
- RFN: 5930
- Chip: 13056
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: po_ConnectionAndSS_Rel:lt_Send_RRC_ConnectionRelease LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4583
- Timestamp: 10:52:59:370_2
- RFN: 5930
- Chip: 17920
- Event: Start Timer
- Source: po_ConnectionAndSS_Rel:lt_RptRcvConnRel LINE 1
- Message Structure:
no details available
- Constraint:
t_Dly (5000 Ms)
- BinaryMessage:

- No.: 4587
- Timestamp: 10:52:59:528_0
- RFN: 5946
- Chip: 7680
- Event: Receive
- PCO: UM
- Message: RLC_UM_DATA_IND
- Source: po_ConnectionAndSS_Rel:lt_RptRcvConnRel LINE 4
- Message Structure:
RLC_UM_DATA_IND
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. IntegrityResult
. uM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00111001011111110001011000001001"
. . . . (IntegerType)rrc_MessageSequenceNumber = 2
. . . UL_DCCH_MessageType
. . . . RRCConnectionReleaseComplete
. . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . FailureCauseWithProtErr
. . . . . laterNonCriticalExtensions
. . . . . . (BitStringType)rrcConnectionReleaseComplete_r3_add_ext = 0
. . . . . . nonCriticalExtensions
- Constraint:
car_RRC_ConnRelCmplUM
- BinaryMessage:
30 0c 02 01 ff 02 01 01 9c bf 8b 04 94 40

- No.: 4588
- Timestamp: 10:52:59:529_0
- RFN: 5946
- Chip: 11776
- Event: Cancel Timer
- Source: po_ConnectionAndSS_Rel:lt_RptRcvConnRel LINE 4
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 4589
- Timestamp: 10:52:59:529_1
- RFN: 5946
- Chip: 12544
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: po_ConnectionAndSS_Rel:lt_RptRcvConnRel LINE 4
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4605
- Timestamp: 10:52:59:536_0
- RFN: 5946
- Chip: 38144
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 01 0a 01 00 05 00

- No.: 4609
- Timestamp: 10:52:59:545_0
- RFN: 5947
- Chip: 35840
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 4612
- Timestamp: 10:52:59:548_0
- RFN: 5948
- Chip: 9216
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 02 0a 01 00 05 00

- No.: 4616
- Timestamp: 10:52:59:557_0
- RFN: 5949
- Chip: 5376
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 4619
- Timestamp: 10:52:59:560_0
- RFN: 5949
- Chip: 15872
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 03 0a 01 00 05 00

- No.: 4623
- Timestamp: 10:52:59:570_0
- RFN: 5950
- Chip: 13824
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 4626
- Timestamp: 10:52:59:573_0
- RFN: 5950
- Chip: 25088
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 04 0a 01 00 05 00

- No.: 4630
- Timestamp: 10:52:59:580_0
- RFN: 5951
- Chip: 15104
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 4636
- Timestamp: 10:52:59:584_0
- RFN: 5951
- Chip: 29952
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = -12
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 f4 0a 01 00 05 00

- No.: 4640
- Timestamp: 10:52:59:589_0
- RFN: 5952
- Chip: 12544
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = -12
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 f4

- No.: 4644
- Timestamp: 10:52:59:598_0
- RFN: 5953
- Chip: 9472
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_CMAC_Rel LINE 1
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
. (RatType)ratType = 0
. configMessage
- Constraint:
cas_MAC_Rel
- BinaryMessage:
30 0b 02 01 ff 02 01 1a 0a 01 00 05 00

- No.: 4648
- Timestamp: 10:52:59:604_0
- RFN: 5953
- Chip: 30464
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_CMAC_Rel LINE 2
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 1a

- No.: 4651
- Timestamp: 10:52:59:611_0
- RFN: 5954
- Chip: 18176
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_CMAC_Rel LINE 1
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
. (RatType)ratType = 0
. configMessage
- Constraint:
cas_MAC_Rel
- BinaryMessage:
30 0b 02 01 ff 02 01 14 0a 01 00 05 00

- No.: 4655
- Timestamp: 10:52:59:616_0
- RFN: 5954
- Chip: 37376
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_CMAC_Rel LINE 2
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 14

- No.: 4658
- Timestamp: 10:52:59:618_0
- RFN: 5955
- Chip: 9728
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Release_REQ
- Source: ts_CPHY_TrChRel LINE 1
- Message Structure:
CPHY_TrCH_Release_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
ca_PHY_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 1a

- No.: 4662
- Timestamp: 10:52:59:625_0
- RFN: 5955
- Chip: 34304
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Release_CNF
- Source: ts_CPHY_TrChRel LINE 2
- Message Structure:
CPHY_TrCH_Release_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
ca_PHY_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 1a

- No.: 4665
- Timestamp: 10:52:59:627_0
- RFN: 5956
- Chip: 5376
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Release_REQ
- Source: ts_CPHY_TrChRel LINE 1
- Message Structure:
CPHY_TrCH_Release_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_PHY_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 4670
- Timestamp: 10:52:59:634_0
- RFN: 5956
- Chip: 29952
- Event: Receive
- PCO: CPHY
- Message: CPHY_Out_of_Sync_IND
- Source: SS_Def LINE 5
- Message Structure:
CPHY_Out_of_Sync_IND
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_OutOfSyncInd
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 4671
- Timestamp: 10:52:59:634_1
- RFN: 5956
- Chip: 33024
- Event: Default
- Source: SS_Def LINE 0
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4672
- Timestamp: 10:52:59:635_0
- RFN: 5956
- Chip: 33792
- Event: Default
- Source: ts_CPHY_TrChRel LINE 2
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4677
- Timestamp: 10:52:59:657_0
- RFN: 5959
- Chip: 4608
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Release_CNF
- Source: ts_CPHY_TrChRel LINE 2
- Message Structure:
CPHY_TrCH_Release_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_PHY_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 4680
- Timestamp: 10:52:59:660_0
- RFN: 5959
- Chip: 15360
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 1a

- No.: 4684
- Timestamp: 10:52:59:667_0
- RFN: 5960
- Chip: 5888
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 1a

- No.: 4687
- Timestamp: 10:52:59:670_0
- RFN: 5960
- Chip: 16640
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 4691
- Timestamp: 10:52:59:696_0
- RFN: 5963
- Chip: 2048
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 4696
- Timestamp: 10:52:59:700_0
- RFN: 5963
- Chip: 15104
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 00 02 01 00 0a 01 00 05 00

- No.: 4700
- Timestamp: 10:52:59:705_0
- RFN: 5963
- Chip: 36864
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 00

- No.: 4703
- Timestamp: 10:52:59:710_0
- RFN: 5964
- Chip: 15616
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_CMAC_Rel LINE 1
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 8
. (RatType)ratType = 0
. configMessage
- Constraint:
cas_MAC_Rel
- BinaryMessage:
30 0b 02 01 00 02 01 08 0a 01 00 05 00

- No.: 4707
- Timestamp: 10:52:59:714_0
- RFN: 5964
- Chip: 32256
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_CMAC_Rel LINE 2
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 8
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 08

- No.: 4710
- Timestamp: 10:52:59:717_0
- RFN: 5965
- Chip: 4352
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Release_REQ
- Source: ts_CPHY_TrChRel LINE 1
- Message Structure:
CPHY_TrCH_Release_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 8
- Constraint:
ca_PHY_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 08

- No.: 4714
- Timestamp: 10:52:59:747_0
- RFN: 5968
- Chip: 6912
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Release_CNF
- Source: ts_CPHY_TrChRel LINE 2
- Message Structure:
CPHY_TrCH_Release_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 8
- Constraint:
ca_PHY_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 08

- No.: 4717
- Timestamp: 10:52:59:750_0
- RFN: 5968
- Chip: 17152
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 7
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 07

- No.: 4721
- Timestamp: 10:52:59:763_0
- RFN: 5969
- Chip: 28928
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 7
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 07

- No.: 4724
- Timestamp: 10:52:59:767_0
- RFN: 5970
- Chip: 6144
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 8
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 08

- No.: 4728
- Timestamp: 10:52:59:812_0
- RFN: 5974
- Chip: 24320
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 8
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 08

- No.: 4731
- Timestamp: 10:52:59:815_0
- RFN: 5974
- Chip: 35584
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -2
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 00 02 01 fe 0a 01 00 05 00

- No.: 4735
- Timestamp: 10:52:59:822_0
- RFN: 5975
- Chip: 22784
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 fe

- No.: 4738
- Timestamp: 10:52:59:826_0
- RFN: 5976
- Chip: 768
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_CMAC_Rel LINE 1
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 5
. (RatType)ratType = 0
. configMessage
- Constraint:
cas_MAC_Rel
- BinaryMessage:
30 0b 02 01 00 02 01 05 0a 01 00 05 00

- No.: 4742
- Timestamp: 10:52:59:833_0
- RFN: 5976
- Chip: 27904
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_CMAC_Rel LINE 2
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 5
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 05

- No.: 4745
- Timestamp: 10:52:59:836_0
- RFN: 5977
- Chip: 256
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Release_REQ
- Source: ts_CPHY_TrChRel LINE 1
- Message Structure:
CPHY_TrCH_Release_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 5
- Constraint:
ca_PHY_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 05

- No.: 4749
- Timestamp: 10:52:59:843_0
- RFN: 5977
- Chip: 27392
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Release_CNF
- Source: ts_CPHY_TrChRel LINE 2
- Message Structure:
CPHY_TrCH_Release_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 5
- Constraint:
ca_PHY_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 05

- No.: 4752
- Timestamp: 10:52:59:846_0
- RFN: 5977
- Chip: 37120
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 6
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 06

- No.: 4756
- Timestamp: 10:52:59:852_0
- RFN: 5978
- Chip: 23808
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 6
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 06

- No.: 4759
- Timestamp: 10:52:59:855_0
- RFN: 5978
- Chip: 34560
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 5
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 05

- No.: 4763
- Timestamp: 10:52:59:863_0
- RFN: 5979
- Chip: 27136
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 5
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 05

- No.: 4768
- Timestamp: 10:52:59:866_0
- RFN: 5980
- Chip: 1536
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 00 02 01 ff 0a 01 00 05 00

- No.: 4772
- Timestamp: 10:52:59:872_0
- RFN: 5980
- Chip: 20992
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 4775
- Timestamp: 10:52:59:875_0
- RFN: 5980
- Chip: 34560
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_CMAC_Rel LINE 1
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 4
. (RatType)ratType = 0
. configMessage
- Constraint:
cas_MAC_Rel
- BinaryMessage:
30 0b 02 01 00 02 01 04 0a 01 00 05 00

- No.: 4779
- Timestamp: 10:52:59:881_0
- RFN: 5981
- Chip: 19712
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_CMAC_Rel LINE 2
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 4
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 04

- No.: 4782
- Timestamp: 10:52:59:884_0
- RFN: 5981
- Chip: 31232
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Release_REQ
- Source: ts_CPHY_TrChRel LINE 1
- Message Structure:
CPHY_TrCH_Release_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 4
- Constraint:
ca_PHY_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 04

- No.: 4786
- Timestamp: 10:52:59:891_0
- RFN: 5982
- Chip: 18176
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Release_CNF
- Source: ts_CPHY_TrChRel LINE 2
- Message Structure:
CPHY_TrCH_Release_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 4
- Constraint:
ca_PHY_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 04

- No.: 4789
- Timestamp: 10:52:59:893_0
- RFN: 5982
- Chip: 28928
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 2
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 02

- No.: 4793
- Timestamp: 10:52:59:899_0
- RFN: 5983
- Chip: 11264
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 2
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 02

- No.: 4796
- Timestamp: 10:52:59:901_0
- RFN: 5983
- Chip: 20736
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 1
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 01

- No.: 4800
- Timestamp: 10:52:59:908_0
- RFN: 5984
- Chip: 6400
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 1
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 01

- No.: 4803
- Timestamp: 10:52:59:910_0
- RFN: 5984
- Chip: 16896
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 4
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 04

- No.: 4807
- Timestamp: 10:52:59:917_0
- RFN: 5985
- Chip: 5376
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 4
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 04

- No.: 4810
- Timestamp: 10:52:59:920_0
- RFN: 5985
- Chip: 16128
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 0
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 00

- No.: 4814
- Timestamp: 10:52:59:926_0
- RFN: 5985
- Chip: 37376
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 0
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 00

- No.: 4831
- Timestamp: 10:52:59:930_1
- RFN: 5986
- Chip: 17152
- Event: Log
- PCO: VERDICT
- Message: PASS
- Source: tc_7_2_3_19 LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage: