- No.: 2
- Timestamp: 21:06:09:778_0
- RFN: 3977
- Chip: 6656
- Event: Start Timer
- Source: tc_7_2_3_26 LINE 1
- Message Structure:
no details available
- Constraint:
t_Guard (300 Sec)
- BinaryMessage:

- No.: 88
- Timestamp: 21:06:09:811_0
- RFN: 3980
- Chip: 15872
- Event: Send
- PCO: Ut
- Message: MMI_CmdReq
- Source: ts_MMI_UE_SwitchOff LINE 1
- Message Structure:
MMI_CmdReq
. (IA5StringType)cmd[-1] = "Please switch off the UE"
- Constraint:
ca_MMI_CmdReq
- BinaryMessage:
50 6c 65 61 73 65 20 73 77 69 74 63 68 20 6f 66 66 20 20 74 68 65 20 55 45

- No.: 92
- Timestamp: 21:06:12:007_0
- RFN: 4200
- Chip: 1280
- Event: Receive
- PCO: Ut
- Message: MMI_CmdCnf
- Source: ts_MMI_UE_SwitchOff LINE 2
- Message Structure:
MMI_CmdCnf
. (BooleanType)result = TRUE
. (IA5StringType)resultString[6] = " OK "
- Constraint:
ca_MMI_CmdCnf
- BinaryMessage:
80 0d 0a 4f 4b 0d 0a

- No.: 96
- Timestamp: 21:06:12:009_0
- RFN: 4200
- Chip: 11264
- Event: Send
- PCO: CPHY
- Message: CPHY_Ini_REQ
- Source: ts_SS_CellCfg:lt_CelllsAlreadyStarted LINE 5
- Message Structure:
CPHY_Ini_REQ
. (CPHY_Ini_REQ)CPHY_Ini_REQ = 0
- Constraint:
cas_InitReqDef
- BinaryMessage:
0a 01 00

- No.: 100
- Timestamp: 21:06:14:050_0
- RFN: 10
- Chip: 16384
- Event: Receive
- PCO: CPHY
- Message: CPHY_Ini_CNF
- Source: ts_SS_CellCfg:lt_CelllsAlreadyStarted LINE 6
- Message Structure:
CPHY_Ini_CNF
- Constraint:
car_IniCnf
- BinaryMessage:
30 02 05 00

- No.: 104
- Timestamp: 21:06:14:053_0
- RFN: 10
- Chip: 27136
- Event: Send
- PCO: CPHY
- Message: CPHY_Cell_Config_REQ
- Source: ts_SS_CellCfg LINE 6
- Message Structure:
CPHY_Cell_Config_REQ
. (IntegerType)cellId = 0
. (IntegerType)tcell = 0
. (IntegerType)sfnOffset = 0
. FrequencyInfo
. . modeSpecificInfo
. . . FrequencyInfoFDD
. . . . (IntegerType)uarfcn_UL = -
. . . . (IntegerType)uarfcn_DL = 10700
. (IntegerType)primaryScramblingCode_SS = 100
. CellTxPowerLevel
. (IntegerType)dLTxAttenuationLevel = 0
- Constraint:
ca_CellCfgReq
- BinaryMessage:
30 19 02 01 00 02 01 00 02 01 00 30 06 30 04 02 02 29 cc 02 01 64 05 00 02 01 00

- No.: 108
- Timestamp: 21:06:14:956_0
- RFN: 100
- Chip: 37120
- Event: Receive
- PCO: CPHY
- Message: CPHY_Cell_Config_CNF
- Source: ts_SS_CellCfg LINE 7
- Message Structure:
CPHY_Cell_Config_CNF
. (IntegerType)cellId = 0
- Constraint:
ca_CellCfgCnf
- BinaryMessage:
30 03 02 01 00

- No.: 120
- Timestamp: 21:06:14:962_0
- RFN: 101
- Chip: 22528
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 3
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 0
. (RatType)ratType = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . PrimaryCPICHInfo
. . . . (IntegerType)dl_TxPower_PCPICH = -60
. . . . (BooleanType)txdiversityIndicator = FALSE
- Constraint:
ca_pCPICH_Info
- BinaryMessage:
30 13 02 01 00 02 01 00 0a 01 00 30 08 30 06 02 01 c4 01 01 00

- No.: 124
- Timestamp: 21:06:14:967_0
- RFN: 102
- Chip: 6400
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 4
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 0
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 00

- No.: 125
- Timestamp: 21:06:14:971_0
- RFN: 102
- Chip: 19456
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 5
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 1
. (RatType)ratType = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . PrimarySCHInfo
. . . . (BooleanType)tstdIndicator = FALSE
. . . . (IntegerType)dl_TxPower = -5
- Constraint:
ca_pSCH_Info
- BinaryMessage:
30 13 02 01 00 02 01 01 0a 01 00 30 08 30 06 01 01 00 02 01 fb

- No.: 129
- Timestamp: 21:06:14:976_0
- RFN: 103
- Chip: 0
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 6
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 1
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 01

- No.: 130
- Timestamp: 21:06:14:979_0
- RFN: 103
- Chip: 12800
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 7
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 2
. (RatType)ratType = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . SecondarySCHInfo
. . . . (BooleanType)tstdIndicator = FALSE
. . . . (IntegerType)dl_TxPower = -5
- Constraint:
ca_sSCH_Info
- BinaryMessage:
30 13 02 01 00 02 01 02 0a 01 00 30 08 30 06 01 01 00 02 01 fb

- No.: 134
- Timestamp: 21:06:15:117_0
- RFN: 117
- Chip: 7168
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 8
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 2
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 02

- No.: 135
- Timestamp: 21:06:15:121_0
- RFN: 117
- Chip: 20480
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 9
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 4
. (RatType)ratType = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . PrimaryCCPCHInfo
. . . . (BooleanType)sttd_Indicator = FALSE
. . . . (IntegerType)dl_TxPower = -2
- Constraint:
ca_pCCPCH_Info
- BinaryMessage:
30 13 02 01 00 02 01 04 0a 01 00 30 08 30 06 01 01 00 02 01 fe

- No.: 139
- Timestamp: 21:06:15:128_0
- RFN: 118
- Chip: 8448
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 10
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 4
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 04

- No.: 140
- Timestamp: 21:06:15:138_0
- RFN: 119
- Chip: 11776
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Config_REQ
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 11
- Message Structure:
CPHY_TrCH_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 4
. (RatType)ratType = 0
. CphyTrchConfigReq
. . SS_ActivationTime
. . ulconnectedTrCHList
. . TFCS
. . dlconnectedTrCHList
. . . CphyTrchConfigReq_setseq_1
. . . . (IntegerType)trchid = 11
. . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 2
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 246
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional = 0
. . . . . . (IntegerType)rateMatchingAttribute = 1
. . . . . . (CRC_Size)crc_Size = 3
. . TFCS
. . . ExplicitTFCS_Configuration
. . . . TFCS_ReconfAdd
. . . . . ctfcSize
. . . . . . ctfc2Bit
. . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . (IntegerType)ctfc2 = 0
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . fdd
. . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 11
. . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
- Constraint:
ca_BCH_InfoActNow
- BinaryMessage:
30 4c 02 01 00 02 01 04 0a 01 00 30 41 05 00 30 23 30 21 02 01 0b 0a 01 02 30 19 30 0c 30 0a 02 02 00 f6 30 02 05 00 05 00 30 09 0a 01 00 02 01 01 0a 01 03 30 18 30 30 15 30 13 02 01 00 30 0e 30 0c 30 30 03 02 01 0b 02 01 0f 02 01 00

- No.: 144
- Timestamp: 21:06:15:146_0
- RFN: 120
- Chip: 2048
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Config_CNF
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 12
- Message Structure:
CPHY_TrCH_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 4
- Constraint:
ca_TrChCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 04

- No.: 145
- Timestamp: 21:06:15:163_0
- RFN: 121
- Chip: 24064
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 13
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 4
. (RatType)ratType = 0
. configMessage
. . CmacConfigReq
. . . SS_ActivationTime
. . . UE_Info
. . . . U_RNTI
. . . . (BitStringType)c_RNTI[16] = -
. . . TrCHInfo
. . . . ulconnectedTrCHList
. . . . TFCS
. . . . dlconnectedTrCHList
. . . . . TrCHInfo_setseq_1
. . . . . . (IntegerType)trchid = 11
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 246
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional = 0
. . . . . . . . (IntegerType)rateMatchingAttribute = 1
. . . . . . . . (CRC_Size)crc_Size = 3
. . . . TFCS
. . . . . ExplicitTFCS_Configuration
. . . . . . TFCS_ReconfAdd
. . . . . . . ctfcSize
. . . . . . . . ctfc2Bit
. . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . (IntegerType)ctfc2 = 0
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 11
. . . . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . TrCH_LogCHMappingList1
. . . . ulconnectedTrCHList
. . . . dlconnectedTrCHList
. . . . . TrCH_LogCHMappingList1_setseq_1
. . . . . . (IntegerType)trchid = 11
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 2
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 0
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 1
. . . . . . . . (IntegerType)rB_Identity = -1
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_CMAC_CfgInfo
- BinaryMessage:
30 70 02 01 00 02 01 04 0a 01 00 30 65 05 00 30 00 30 3c 30 20 30 1e 02 01 0b 30 19 30 0c 30 0a 02 02 00 f6 30 02 05 00 05 00 30 09 0a 01 00 02 01 01 0a 01 03 30 18 30 30 15 30 13 02 01 00 30 0e 30 0c 30 30 03 02 01 0b 02 01 0f 02 01 00 30 21 30 1f 30 1d 02 01 0b 30 18 30 16 30 11 0a 01 00 0a 01 02 02 01 01 0a 01 00 05 00 02 01 01 02 01 ff

- No.: 149
- Timestamp: 21:06:15:174_0
- RFN: 122
- Chip: 29952
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 14
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 4
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 04

- No.: 157
- Timestamp: 21:06:15:180_0
- RFN: 123
- Chip: 14592
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_PCH_FACH_CCCH_Cfg LINE 3
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 5
. (RatType)ratType = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . SecondaryCCPCHInfo
. . . . (IntegerType)scramblingCode = 0
. . . . SF256_AndCodeNumber
. . . . . (IntegerType)sf64 = 1
. . . . (IntegerType)sCCPCHSlotFormat = 8
. . . . (IntegerType)timingOffset = 0
. . . . (PositionFixedOrFlexible)positionFixedOrFlexible = 1
. . . . (BooleanType)sttd_Indicator = FALSE
. . . . (IntegerType)dl_TxPower = -2
. . . . (IntegerType)powerOffsetOfTFCI_PO1 = 6
. . . . (IntegerType)powerOffsetOfPILOT_PO3 = 6
- Constraint:
ca_sCCPCH_Info
- BinaryMessage:
30 28 02 01 00 02 01 05 0a 01 00 30 1d 30 1b 02 01 00 02 01 01 02 01 08 02 01 00 0a 01 01 01 01 00 02 01 fe 02 01 06 02 01 06

- No.: 161
- Timestamp: 21:06:15:187_0
- RFN: 124
- Chip: 3328
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_PCH_FACH_CCCH_Cfg LINE 4
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 5
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 05

- No.: 162
- Timestamp: 21:06:15:213_0
- RFN: 126
- Chip: 26880
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Config_REQ
- Source: ts_SS_PCH_FACH_CCCH_Cfg LINE 5
- Message Structure:
CPHY_TrCH_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 5
. (RatType)ratType = 0
. CphyTrchConfigReq
. . SS_ActivationTime
. . ulconnectedTrCHList
. . TFCS
. . dlconnectedTrCHList
. . . CphyTrchConfigReq_setseq_1
. . . . (IntegerType)trchid = 12
. . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 3
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 240
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional = 0
. . . . . . (IntegerType)rateMatchingAttribute = 230
. . . . . . (CRC_Size)crc_Size = 3
. . . CphyTrchConfigReq_setseq_1
. . . . (IntegerType)trchid = 13
. . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 1
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 168
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . (IntegerType)small = 2
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional = 0
. . . . . . (IntegerType)rateMatchingAttribute = 220
. . . . . . (CRC_Size)crc_Size = 3
. . . CphyTrchConfigReq_setseq_1
. . . . (IntegerType)trchid = 14
. . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 1
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 360
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . (IntegerType)rateMatchingAttribute = 130
. . . . . . (CRC_Size)crc_Size = 3
. . TFCS
. . . ExplicitTFCS_Configuration
. . . . TFCS_ReconfAdd
. . . . . ctfcSize
. . . . . . ctfc4Bit
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 0
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 1
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 2
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 3
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 4
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 5
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 6
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 8
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . fdd
. . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 11
. . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
- Constraint:
ca_PCH_2_FACH_InfoActNow
- BinaryMessage:
30 81 e4 02 01 00 02 01 05 0a 01 00 30 81 d8 05 00 30 74 30 24 02 01 0c 0a 01 03 30 1c 30 0e 30 0c 02 02 00 f0 30 04 05 00 05 00 05 00 30 0a 0a 01 00 02 02 00 e6 0a 01 03 30 27 02 01 0d 0a 01 01 30 1f 30 11 30 0f 02 02 00 a8 30 07 05 00 05 00 02 01 02 05 00 30 0a 0a 01 00 02 02 00 dc 0a 01 03 30 23 02 01 0e 0a 01 01 30 1b 30 0e 30 0c 02 02 01 68 30 04 05 00 05 00 05 00 30 09 05 00 02 02 00 82 0a 01 03 30 5e 30 30 5b 30 08 02 01 00 30 03 02 01 00 30 08 02 01 01 30 03 02 01 00 30 08 02 01 02 30 03 02 01 00 30 08 02 01 03 30 03 02 01 00 30 08 02 01 04 30 03 02 01 00 30 08 02 01 05 30 03 02 01 00 30 08 02 01 06 30 03 02 01 00 30 13 02 01 08 30 0e 30 0c 30 30 03 02 01 0b 02 01 0f 02 01 00

- No.: 166
- Timestamp: 21:06:15:224_0
- RFN: 127
- Chip: 32256
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Config_CNF
- Source: ts_SS_PCH_FACH_CCCH_Cfg LINE 6
- Message Structure:
CPHY_TrCH_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 5
- Constraint:
ca_TrChCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 05

- No.: 167
- Timestamp: 21:06:15:265_0
- RFN: 131
- Chip: 33024
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_SS_PCH_FACH_CCCH_Cfg LINE 7
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 5
. (RatType)ratType = 0
. configMessage
. . CmacConfigReq
. . . SS_ActivationTime
. . . UE_Info
. . . . U_RNTI
. . . . (BitStringType)c_RNTI[16] = -
. . . TrCHInfo
. . . . ulconnectedTrCHList
. . . . TFCS
. . . . dlconnectedTrCHList
. . . . . TrCHInfo_setseq_1
. . . . . . (IntegerType)trchid = 12
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 240
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional = 0
. . . . . . . . (IntegerType)rateMatchingAttribute = 230
. . . . . . . . (CRC_Size)crc_Size = 3
. . . . . TrCHInfo_setseq_1
. . . . . . (IntegerType)trchid = 13
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 168
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . (IntegerType)small = 2
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional = 0
. . . . . . . . (IntegerType)rateMatchingAttribute = 220
. . . . . . . . (CRC_Size)crc_Size = 3
. . . . . TrCHInfo_setseq_1
. . . . . . (IntegerType)trchid = 14
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 360
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . (IntegerType)rateMatchingAttribute = 130
. . . . . . . . (CRC_Size)crc_Size = 3
. . . . TFCS
. . . . . ExplicitTFCS_Configuration
. . . . . . TFCS_ReconfAdd
. . . . . . . ctfcSize
. . . . . . . . ctfc4Bit
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 0
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 1
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 2
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 3
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 4
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 5
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 6
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 8
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 11
. . . . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . TrCH_LogCHMappingList1
. . . . ulconnectedTrCHList
. . . . dlconnectedTrCHList
. . . . . TrCH_LogCHMappingList1_setseq_1
. . . . . . (IntegerType)trchid = 12
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 3
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 1
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 1
. . . . . . . . (IntegerType)rB_Identity = -2
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . TrCH_LogCHMappingList1_setseq_1
. . . . . . (IntegerType)trchid = 13
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 1
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 5
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 2
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 1
. . . . . . . . (IntegerType)rB_Identity = 0
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_CMAC_CfgInfo
- BinaryMessage:
30 82 01 23 02 01 00 02 01 05 0a 01 00 30 82 01 16 05 00 30 00 30 81 cd 30 6b 30 21 02 01 0c 30 1c 30 0e 30 0c 02 02 00 f0 30 04 05 00 05 00 05 00 30 0a 0a 01 00 02 02 00 e6 0a 01 03 30 24 02 01 0d 30 1f 30 11 30 0f 02 02 00 a8 30 07 05 00 05 00 02 01 02 05 00 30 0a 0a 01 00 02 02 00 dc 0a 01 03 30 20 02 01 0e 30 1b 30 0e 30 0c 02 02 01 68 30 04 05 00 05 00 05 00 30 09 05 00 02 02 00 82 0a 01 03 30 5e 30 30 5b 30 08 02 01 00 30 03 02 01 00 30 08 02 01 01 30 03 02 01 00 30 08 02 01 02 30 03 02 01 00 30 08 02 01 03 30 03 02 01 00 30 08 02 01 04 30 03 02 01 00 30 08 02 01 05 30 03 02 01 00 30 08 02 01 06 30 03 02 01 00 30 13 02 01 08 30 0e 30 0c 30 30 03 02 01 0b 02 01 0f 02 01 00 30 40 30 3e 30 1d 02 01 0c 30 18 30 16 30 11 0a 01 00 0a 01 03 02 01 01 0a 01 01 05 00 02 01 01 02 01 fe 30 1d 02 01 0d 30 18 30 16 30 11 0a 01 00 0a 01 01 02 01 05 0a 01 02 05 00 02 01 01 02 01 00

- No.: 171
- Timestamp: 21:06:15:312_0
- RFN: 136
- Chip: 24832
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_SS_PCH_FACH_CCCH_Cfg LINE 8
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 5
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 05

- No.: 172
- Timestamp: 21:06:15:317_0
- RFN: 137
- Chip: 3584
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_PCH_FACH_CCCH_Cfg LINE 9
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 6
. (RatType)ratType = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . PICHInfo
. . . . PICH_Info
. . . . . fdd
. . . . . . (IntegerType)channelisationCode256 = 2
. . . . . . (PI_CountPerFrame)pi_CountPerFrame = 0
. . . . . . (BooleanType)sttd_Indicator = FALSE
. . . . (IntegerType)dl_TxPower = -5
- Constraint:
ca_PICH_Info
- BinaryMessage:
30 1c 02 01 00 02 01 06 0a 01 00 30 11 30 0f 30 30 09 02 01 02 0a 01 00 01 01 00 02 01 fb

- No.: 176
- Timestamp: 21:06:15:324_0
- RFN: 137
- Chip: 30720
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_PCH_FACH_CCCH_Cfg LINE 10
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 6
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 06

- No.: 184
- Timestamp: 21:06:15:329_0
- RFN: 138
- Chip: 14336
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_RACH_CCCH_Cfg LINE 3
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 7
. (RatType)ratType = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . AICHInfo
. . . . AICH_Info
. . . . . (IntegerType)channelisationCode256 = 3
. . . . . (BooleanType)sttd_Indicator = FALSE
. . . . . (AICH_TransmissionTiming)aich_TransmissionTiming = 0
. . . . (IntegerType)dl_TxPower = -5
- Constraint:
ca_AichInfo
- BinaryMessage:
30 1b 02 01 00 02 01 07 0a 01 00 30 10 30 0e 30 09 02 01 03 01 01 00 0a 01 00 02 01 fb

- No.: 188
- Timestamp: 21:06:15:337_0
- RFN: 139
- Chip: 3840
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_RACH_CCCH_Cfg LINE 4
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 7
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 07

- No.: 189
- Timestamp: 21:06:15:341_0
- RFN: 139
- Chip: 21504
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_RACH_CCCH_Cfg LINE 5
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 8
. (RatType)ratType = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . PRACHInfo
. . . . fdd_tdd
. . . . . fdd
. . . . . . (BitStringType)preambleSignature[16] = "0000000011111111"
. . . . . . (SF_PRACH)spreadingFactorForDataPart = 1
. . . . . . (IntegerType)preambleScramblingCode = 0
. . . . . . (PuncturingLimit)puncturingLimit = 15
. . . . . . (BitStringType)accessSlot[12] = "111111111111"
- Constraint:
ca_PRACH_Info
- BinaryMessage:
30 23 02 01 00 02 01 08 0a 01 00 30 18 30 16 30 30 13 03 03 00 00 ff 0a 01 01 02 01 00 0a 01 0f 03 03 04 ff f0

- No.: 193
- Timestamp: 21:06:15:351_0
- RFN: 140
- Chip: 20992
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_RACH_CCCH_Cfg LINE 6
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 8
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 08

- No.: 194
- Timestamp: 21:06:15:362_0
- RFN: 141
- Chip: 24576
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Config_REQ
- Source: ts_SS_RACH_CCCH_Cfg LINE 7
- Message Structure:
CPHY_TrCH_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 8
. (RatType)ratType = 0
. CphyTrchConfigReq
. . SS_ActivationTime
. . ulconnectedTrCHList
. . . CphyTrchConfigReq_setseq_0
. . . . (IntegerType)trchid = 15
. . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 1
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 168
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 360
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional = 0
. . . . . . (IntegerType)rateMatchingAttribute = 150
. . . . . . (CRC_Size)crc_Size = 3
. . TFCS
. . . ExplicitTFCS_Configuration
. . . . TFCS_ReconfAdd
. . . . . ctfcSize
. . . . . . ctfc2Bit
. . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . (IntegerType)ctfc2 = 0
. . . . . . . . PowerOffsetInformation
. . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . (IntegerType)ctfc2 = 1
. . . . . . . . PowerOffsetInformation
. . dlconnectedTrCHList
. . TFCS
- Constraint:
cab_RACH_InfoActNow
- BinaryMessage:
30 4e 02 01 00 02 01 08 0a 01 00 30 43 05 00 30 30 30 2e 02 01 0f 0a 01 01 30 26 30 18 30 0a 02 02 00 a8 30 02 05 00 05 00 30 0a 02 02 01 68 30 02 05 00 05 00 30 0a 0a 01 00 02 02 00 96 0a 01 03 30 0d 30 30 0a 30 03 02 01 00 30 03 02 01 01

- No.: 198
- Timestamp: 21:06:15:371_0
- RFN: 142
- Chip: 21760
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Config_CNF
- Source: ts_SS_RACH_CCCH_Cfg LINE 8
- Message Structure:
CPHY_TrCH_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 8
- Constraint:
ca_TrChCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 08

- No.: 199
- Timestamp: 21:06:15:389_0
- RFN: 144
- Chip: 12032
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_SS_RACH_CCCH_Cfg LINE 9
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 8
. (RatType)ratType = 0
. configMessage
. . CmacConfigReq
. . . SS_ActivationTime
. . . UE_Info
. . . . U_RNTI
. . . . (BitStringType)c_RNTI[16] = -
. . . TrCHInfo
. . . . ulconnectedTrCHList
. . . . . TrCHInfo_setseq_0
. . . . . . (IntegerType)trchid = 15
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 168
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 360
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional = 0
. . . . . . . . (IntegerType)rateMatchingAttribute = 150
. . . . . . . . (CRC_Size)crc_Size = 3
. . . . TFCS
. . . . . ExplicitTFCS_Configuration
. . . . . . TFCS_ReconfAdd
. . . . . . . ctfcSize
. . . . . . . . ctfc2Bit
. . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . (IntegerType)ctfc2 = 0
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . (IntegerType)ctfc2 = 1
. . . . . . . . . . PowerOffsetInformation
. . . . dlconnectedTrCHList
. . . . TFCS
. . . TrCH_LogCHMappingList1
. . . . ulconnectedTrCHList
. . . . . TrCH_LogCHMappingList1_setseq_0
. . . . . . (IntegerType)trchid = 15
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 1
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 5
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 2
. . . . . . . . (IntegerType)rB_Identity = 0
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . dlconnectedTrCHList
- Constraint:
ca_CMAC_CfgInfo
- BinaryMessage:
30 6d 02 01 00 02 01 08 0a 01 00 30 62 05 00 30 00 30 3e 30 2d 30 2b 02 01 0f 30 26 30 18 30 0a 02 02 00 a8 30 02 05 00 05 00 30 0a 02 02 01 68 30 02 05 00 05 00 30 0a 0a 01 00 02 02 00 96 0a 01 03 30 0d 30 30 0a 30 03 02 01 00 30 03 02 01 01 30 1c 30 1a 30 18 02 01 0f 30 13 30 11 30 0c 0a 01 00 0a 01 01 02 01 05 0a 01 02 02 01 00

- No.: 200
- Timestamp: 21:06:15:395_0
- RFN: 144
- Chip: 35328
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_SS_RACH_CCCH_Cfg LINE 10
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 8
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 08

- No.: 237
- Timestamp: 21:06:15:414_0
- RFN: 146
- Chip: 31232
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_1DCH_DCCH_Cfg LINE 4
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
. (RatType)ratType = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . DPCHInfo
. . . . UL_DPCH_Info
. . . . DL_DPCHInfo
. . . . . DL_CommonInformation
. . . . . . DL_DPCH_InfoCommon
. . . . . . . cfnHandling
. . . . . . . . initialise
. . . . . . . . . (IntegerType)cfntargetsfnframeoffset = -
. . . . . . . modeSpecificInfo
. . . . . . . . fdd
. . . . . . . . . DL_DPCH_PowerControlInfo
. . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . fdd
. . . . . . . . . . . . (DPC_Mode)dpc_Mode = 0
. . . . . . . . . (IntegerType)powerOffsetPilot_pdpdch = 0
. . . . . . . . . Dl_rate_matching_restriction
. . . . . . . . . SF512_AndPilot
. . . . . . . . . . (PilotBits128)sfd128 = 0
. . . . . . . . . (PositionFixedOrFlexible)positionFixedOrFlexible = 0
. . . . . . . . . (BooleanType)tfci_Existence = FALSE
. . . . . . modeSpecificInfo
. . . . . . . fdd
. . . . . . . . (IntegerType)defaultDPCH_OffsetValue = 0
. . . . . . . . DPCH_CompressedModeInfo
. . . . . . . . (TX_DiversityMode)tx_DiversityMode = 0
. . . . . . . . SSDT_Information
. . . . . DL_DPCH_InfoPerRL
. . . . . . fdd
. . . . . . . (PCPICH_UsageForChannelEst)pCPICH_UsageForChannelEst = 0
. . . . . . . (IntegerType)dpch_FrameOffset = 0
. . . . . . . SecondaryCPICH_Info
. . . . . . . DL_ChannelisationCodeList
. . . . . . . . DL_ChannelisationCode
. . . . . . . . . (IntegerType)secondaryScramblingCode = 1
. . . . . . . . . SF512_AndCodeNumber
. . . . . . . . . . (IntegerType)sf128 = 0
. . . . . . . . . (ScramblingCodeChange)scramblingCodeChange = -
. . . . . . . (IntegerType)tpc_CombinationIndex = 0
. . . . . . . (SSDT_CellIdentity)ssdt_CellIdentity = -
. . . . . . . (ClosedLoopTimingAdjMode)closedLoopTimingAdjMode = -
. . . . . (IntegerType)powerOffsetOfTFCI_PO1 = 0
. . . . . (IntegerType)powerOffsetOfTPC_PO2 = 0
. . . . . (IntegerType)powerOffsetOfPILOT_PO3 = 0
. . . . . (IntegerType)dl_TxPower = -5
. . . . . (IntegerType)dl_TxPowerMax = 15
. . . . . (IntegerType)dl_TxPowerMin = -35
- Constraint:
ca_DL_DPCH_Info
- BinaryMessage:
30 5e 02 01 00 02 01 1a 0a 01 00 30 53 30 51 30 4f 30 25 30 1a 30 30 00 30 30 14 30 06 30 30 03 0a 01 00 02 01 00 0a 01 00 0a 01 00 01 01 00 30 30 06 02 01 00 0a 01 00 30 30 13 0a 01 00 02 01 00 30 08 30 06 02 01 01 02 01 00 02 01 00 02 01 00 02 01 00 02 01 00 02 01 fb 02 01 0f 02 01 dd

- No.: 241
- Timestamp: 21:06:15:423_0
- RFN: 147
- Chip: 29696
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_1DCH_DCCH_Cfg LINE 5
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 1a

- No.: 242
- Timestamp: 21:06:15:435_0
- RFN: 148
- Chip: 37120
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Config_REQ
- Source: ts_SS_1DCH_DCCH_Cfg LINE 6
- Message Structure:
CPHY_TrCH_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
. (RatType)ratType = 0
. CphyTrchConfigReq
. . SS_ActivationTime
. . ulconnectedTrCHList
. . TFCS
. . dlconnectedTrCHList
. . . CphyTrchConfigReq_setseq_1
. . . . (IntegerType)trchid = 10
. . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 148
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional = 1
. . . . . . (IntegerType)rateMatchingAttribute = 192
. . . . . . (CRC_Size)crc_Size = 3
. . TFCS
. . . ExplicitTFCS_Configuration
. . . . TFCS_ReconfAdd
. . . . . ctfcSize
. . . . . . ctfc2Bit
. . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . (IntegerType)ctfc2 = 0
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . (IntegerType)ctfc2 = 1
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . fdd
. . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 11
. . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
- Constraint:
ca_DCH_148_TTI_10_DL_InfoActNow
- BinaryMessage:
30 59 02 01 00 02 01 1a 0a 01 00 30 4e 05 00 30 26 30 24 02 01 0a 0a 01 00 30 1c 30 0e 30 0c 02 02 00 94 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 c0 0a 01 03 30 22 30 30 1f 30 08 02 01 00 30 03 02 01 00 30 13 02 01 01 30 0e 30 0c 30 30 03 02 01 0b 02 01 0f 02 01 00

- No.: 246
- Timestamp: 21:06:15:445_0
- RFN: 149
- Chip: 35840
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Config_CNF
- Source: ts_SS_1DCH_DCCH_Cfg LINE 7
- Message Structure:
CPHY_TrCH_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
ca_TrChCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 1a

- No.: 247
- Timestamp: 21:06:15:478_0
- RFN: 153
- Chip: 5888
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_SS_1DCH_DCCH_Cfg LINE 8
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
. (RatType)ratType = 0
. configMessage
. . CmacConfigReq
. . . SS_ActivationTime
. . . UE_Info
. . . . U_RNTI
. . . . (BitStringType)c_RNTI[16] = -
. . . TrCHInfo
. . . . ulconnectedTrCHList
. . . . TFCS
. . . . dlconnectedTrCHList
. . . . . TrCHInfo_setseq_1
. . . . . . (IntegerType)trchid = 10
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 148
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . (IntegerType)rateMatchingAttribute = 192
. . . . . . . . (CRC_Size)crc_Size = 3
. . . . TFCS
. . . . . ExplicitTFCS_Configuration
. . . . . . TFCS_ReconfAdd
. . . . . . . ctfcSize
. . . . . . . . ctfc2Bit
. . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . (IntegerType)ctfc2 = 0
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . (IntegerType)ctfc2 = 1
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 11
. . . . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . TrCH_LogCHMappingList1
. . . . ulconnectedTrCHList
. . . . dlconnectedTrCHList
. . . . . TrCH_LogCHMappingList1_setseq_1
. . . . . . (IntegerType)trchid = 10
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 1
. . . . . . . . (IntegerType)rB_Identity = 1
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 2
. . . . . . . . (IntegerType)rB_Identity = 2
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 3
. . . . . . . . (IntegerType)rB_Identity = 3
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 4
. . . . . . . . (IntegerType)rB_Identity = 4
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_CMAC_CfgInfo
- BinaryMessage:
30 81 c6 02 01 ff 02 01 1a 0a 01 00 30 81 ba 05 00 30 00 30 49 30 23 30 21 02 01 0a 30 1c 30 0e 30 0c 02 02 00 94 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 c0 0a 01 03 30 22 30 30 1f 30 08 02 01 00 30 03 02 01 00 30 13 02 01 01 30 0e 30 0c 30 30 03 02 01 0b 02 01 0f 02 01 00 30 69 30 67 30 65 02 01 0a 30 60 30 16 30 11 0a 01 00 0a 01 00 02 01 01 0a 01 04 05 00 02 01 01 02 01 01 30 16 30 11 0a 01 00 0a 01 00 02 01 02 0a 01 04 05 00 02 01 02 02 01 02 30 16 30 11 0a 01 00 0a 01 00 02 01 03 0a 01 04 05 00 02 01 03 02 01 03 30 16 30 11 0a 01 00 0a 01 00 02 01 04 0a 01 04 05 00 02 01 04 02 01 04

- No.: 251
- Timestamp: 21:06:15:497_0
- RFN: 155
- Chip: 3840
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_SS_1DCH_DCCH_Cfg LINE 9
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 1a

- No.: 252
- Timestamp: 21:06:15:503_0
- RFN: 155
- Chip: 26368
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_1DCH_DCCH_Cfg LINE 10
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
. (RatType)ratType = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . DPCHInfo
. . . . UL_DPCH_Info
. . . . . UL_DPCH_PowerControlInfo
. . . . . . fdd
. . . . . . . (IntegerType)dpcch_PowerOffset = -40
. . . . . . . (IntegerType)pc_Preamble = 1
. . . . . . . (IntegerType)sRB_delay = 7
. . . . . . . PowerControlAlgorithm
. . . . . . . . (IntegerType)algorithm1 = 1
. . . . . modeSpecificInfo
. . . . . . fdd
. . . . . . . (ScramblingCodeType)scramblingCodeType = 1
. . . . . . . (IntegerType)scramblingCode = 0
. . . . . . . (IntegerType)numberOfDPDCH = -
. . . . . . . (SpreadingFactor)spreadingFactor = 4
. . . . . . . (BooleanType)tfci_Existence = TRUE
. . . . . . . (IntegerType)numberOfFBI_Bits = -
. . . . . . . (PuncturingLimit)puncturingLimit = 15
. . . . DL_DPCHInfo
- Constraint:
ca_UL_DPCH_Info
- BinaryMessage:
30 30 02 01 00 02 01 14 0a 01 00 30 25 30 23 30 21 30 30 0c 02 01 d8 02 01 01 02 01 07 02 01 01 30 30 0f 0a 01 01 02 01 00 0a 01 04 01 01 ff 0a 01 0f

- No.: 256
- Timestamp: 21:06:15:512_0
- RFN: 156
- Chip: 23808
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_1DCH_DCCH_Cfg LINE 11
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 257
- Timestamp: 21:06:15:522_0
- RFN: 157
- Chip: 24064
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Config_REQ
- Source: ts_SS_1DCH_DCCH_Cfg LINE 12
- Message Structure:
CPHY_TrCH_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
. (RatType)ratType = 0
. CphyTrchConfigReq
. . SS_ActivationTime
. . ulconnectedTrCHList
. . . CphyTrchConfigReq_setseq_0
. . . . (IntegerType)trchid = 5
. . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 148
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional = 1
. . . . . . (IntegerType)rateMatchingAttribute = 192
. . . . . . (CRC_Size)crc_Size = 3
. . TFCS
. . . ExplicitTFCS_Configuration
. . . . TFCS_ReconfAdd
. . . . . ctfcSize
. . . . . . ctfc2Bit
. . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . (IntegerType)ctfc2 = 0
. . . . . . . . PowerOffsetInformation
. . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . (IntegerType)ctfc2 = 1
. . . . . . . . PowerOffsetInformation
. . dlconnectedTrCHList
. . TFCS
- Constraint:
ca_DCH_148_TTI_10_UL_InfoActNow
- BinaryMessage:
30 44 02 01 00 02 01 14 0a 01 00 30 39 05 00 30 26 30 24 02 01 05 0a 01 00 30 1c 30 0e 30 0c 02 02 00 94 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 c0 0a 01 03 30 0d 30 30 0a 30 03 02 01 00 30 03 02 01 01

- No.: 261
- Timestamp: 21:06:15:532_0
- RFN: 158
- Chip: 24320
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Config_CNF
- Source: ts_SS_1DCH_DCCH_Cfg LINE 13
- Message Structure:
CPHY_TrCH_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_TrChCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 262
- Timestamp: 21:06:15:564_0
- RFN: 161
- Chip: 30464
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_SS_1DCH_DCCH_Cfg LINE 14
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
. (RatType)ratType = 0
. configMessage
. . CmacConfigReq
. . . SS_ActivationTime
. . . UE_Info
. . . . U_RNTI
. . . . (BitStringType)c_RNTI[16] = -
. . . TrCHInfo
. . . . ulconnectedTrCHList
. . . . . TrCHInfo_setseq_0
. . . . . . (IntegerType)trchid = 5
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 148
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . (IntegerType)rateMatchingAttribute = 192
. . . . . . . . (CRC_Size)crc_Size = 3
. . . . TFCS
. . . . . ExplicitTFCS_Configuration
. . . . . . TFCS_ReconfAdd
. . . . . . . ctfcSize
. . . . . . . . ctfc2Bit
. . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . (IntegerType)ctfc2 = 0
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . (IntegerType)ctfc2 = 1
. . . . . . . . . . PowerOffsetInformation
. . . . dlconnectedTrCHList
. . . . TFCS
. . . TrCH_LogCHMappingList1
. . . . ulconnectedTrCHList
. . . . . TrCH_LogCHMappingList1_setseq_0
. . . . . . (IntegerType)trchid = 5
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . (IntegerType)rB_Identity = 1
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . (IntegerType)rB_Identity = 2
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . (IntegerType)rB_Identity = 3
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . (IntegerType)rB_Identity = 4
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . dlconnectedTrCHList
- Constraint:
ca_CMAC_CfgInfo
- BinaryMessage:
30 81 9d 02 01 ff 02 01 14 0a 01 00 30 81 91 05 00 30 00 30 34 30 23 30 21 02 01 05 30 1c 30 0e 30 0c 02 02 00 94 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 c0 0a 01 03 30 0d 30 30 0a 30 03 02 01 00 30 03 02 01 01 30 55 30 53 30 51 02 01 05 30 4c 30 11 30 0c 0a 01 00 0a 01 00 02 01 01 0a 01 04 02 01 01 30 11 30 0c 0a 01 00 0a 01 00 02 01 02 0a 01 04 02 01 02 30 11 30 0c 0a 01 00 0a 01 00 02 01 03 0a 01 04 02 01 03 30 11 30 0c 0a 01 00 0a 01 00 02 01 04 0a 01 04 02 01 04

- No.: 266
- Timestamp: 21:06:15:585_0
- RFN: 163
- Chip: 36352
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_SS_1DCH_DCCH_Cfg LINE 15
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 14

- No.: 269
- Timestamp: 21:06:15:591_0
- RFN: 164
- Chip: 20224
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB_BCCH_BCH_Cfg LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 246
. . . . . UL_RLC_Mode
. . . . . . UL_TM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . (BooleanType)segmentationIndication = FALSE
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = -
. . . . (IntegerType)dLlogicalChannelIdentity = 1
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_BCCH_Info
- BinaryMessage:
30 1d 02 01 00 02 01 ff 0a 01 00 30 12 30 0b 30 09 02 02 00 f6 30 03 01 01 00 30 03 02 01 01

- No.: 273
- Timestamp: 21:06:15:597_0
- RFN: 165
- Chip: 3584
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB_BCCH_BCH_Cfg LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 276
- Timestamp: 21:06:15:602_0
- RFN: 165
- Chip: 24832
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB_PCCH_Cfg LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -2
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 240
. . . . . UL_RLC_Mode
. . . . . . UL_TM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . (BooleanType)segmentationIndication = FALSE
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = -
. . . . (IntegerType)dLlogicalChannelIdentity = 1
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_PCCH_Info
- BinaryMessage:
30 1d 02 01 00 02 01 fe 0a 01 00 30 12 30 0b 30 09 02 02 00 f0 30 03 01 01 00 30 03 02 01 01

- No.: 280
- Timestamp: 21:06:15:607_0
- RFN: 166
- Chip: 5120
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB_PCCH_Cfg LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 fe

- No.: 283
- Timestamp: 21:06:15:613_0
- RFN: 166
- Chip: 27392
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB0_Cfg LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 152
. . . . . UL_RLC_Mode
. . . . . . UL_UM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (NoExplicitDiscard)timerBasedNoExplicit = 9
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = -
. . . . (IntegerType)dLlogicalChannelIdentity = 5
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_UM_DL_Info
- BinaryMessage:
30 1d 02 01 00 02 01 00 0a 01 00 30 12 30 0b 30 09 02 02 00 98 30 03 0a 01 09 30 03 02 01 05

- No.: 287
- Timestamp: 21:06:15:623_0
- RFN: 167
- Chip: 29440
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB0_Cfg LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 00

- No.: 288
- Timestamp: 21:06:15:630_0
- RFN: 168
- Chip: 14848
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB0_Cfg LINE 3
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_TM_RLC_Mode
. . . . . . (BooleanType)segmentationIndication = TRUE
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 166
. . . . . UL_RLC_Mode
. . . . . . UL_TM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . (BooleanType)segmentationIndication = TRUE
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = 5
. . . . (IntegerType)dLlogicalChannelIdentity = -
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_TM_UL_Info
- BinaryMessage:
30 22 02 01 00 02 01 00 0a 01 00 30 17 30 10 30 03 01 01 ff 30 09 02 02 00 a6 30 03 01 01 ff 30 03 02 01 05

- No.: 292
- Timestamp: 21:06:15:638_0
- RFN: 169
- Chip: 7168
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB0_Cfg LINE 4
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 00

- No.: 295
- Timestamp: 21:06:15:645_0
- RFN: 169
- Chip: 34560
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 136
. . . . . UL_RLC_Mode
. . . . . . UL_UM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (NoExplicitDiscard)timerBasedNoExplicit = 9
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = 1
. . . . (IntegerType)dLlogicalChannelIdentity = 1
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_UM_Info
- BinaryMessage:
30 22 02 01 ff 02 01 01 0a 01 00 30 17 30 0d 05 00 30 09 02 02 00 88 30 03 0a 01 09 30 06 02 01 01 02 01 01

- No.: 299
- Timestamp: 21:06:15:655_0
- RFN: 170
- Chip: 35072
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 300
- Timestamp: 21:06:15:664_0
- RFN: 171
- Chip: 32512
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 3
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . (TimerEPC)timerEPC = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . (TimerRST)timerRST = 9
. . . . . . . (MaxRST)max_RST = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = 2
. . . . (IntegerType)dLlogicalChannelIdentity = 2
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 02 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 27 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 02 02 01 02

- No.: 304
- Timestamp: 21:06:15:684_0
- RFN: 173
- Chip: 31232
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 4
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 305
- Timestamp: 21:06:15:693_0
- RFN: 174
- Chip: 28416
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 5
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . (TimerEPC)timerEPC = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . (TimerRST)timerRST = 9
. . . . . . . (MaxRST)max_RST = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = 3
. . . . (IntegerType)dLlogicalChannelIdentity = 3
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 03 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 27 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 03 02 01 03

- No.: 309
- Timestamp: 21:06:15:714_0
- RFN: 176
- Chip: 30976
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 6
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 310
- Timestamp: 21:06:15:723_0
- RFN: 177
- Chip: 27648
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 7
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . (TimerEPC)timerEPC = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . (TimerRST)timerRST = 9
. . . . . . . (MaxRST)max_RST = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = 4
. . . . (IntegerType)dLlogicalChannelIdentity = 4
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 04 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 27 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 04 02 01 04

- No.: 314
- Timestamp: 21:06:15:744_0
- RFN: 179
- Chip: 32512
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 8
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 355
- Timestamp: 21:06:15:790_0
- RFN: 184
- Chip: 14848
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 27
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 1b

- No.: 360
- Timestamp: 21:06:15:795_0
- RFN: 184
- Chip: 32768
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendNoSegDefSchedul LINE 2
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 361
- Timestamp: 21:06:15:798_0
- RFN: 185
- Chip: 8704
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendNoSegDefSchedul LINE 3
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 08 02 01 00 02 01 ff 00 00

- No.: 369
- Timestamp: 21:06:15:809_0
- RFN: 186
- Chip: 10496
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 11
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 0b

- No.: 374
- Timestamp: 21:06:15:816_0
- RFN: 186
- Chip: 36864
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB1 LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 375
- Timestamp: 21:06:15:821_0
- RFN: 187
- Chip: 19968
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB1 LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 1
. . . . . . . (BitStringType)sib_Data_variable[-1] = "1100010000000000000001011000100000101000000010100001000111100000000101000000000000000000000011000111010000"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 2
. . . . . . . (BitStringType)sib_Data_variable[-1] = "10000000000000000001"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 1c 02 01 00 02 01 ff 00 0e 21 69 c4 00 05 88 28 0a 11 e0 14 00 00 0c 74 04 27 00 00 20

- No.: 388
- Timestamp: 21:06:15:831_0
- RFN: 188
- Chip: 19968
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 11
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 0b

- No.: 393
- Timestamp: 21:06:15:836_0
- RFN: 188
- Chip: 37376
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB2 LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 394
- Timestamp: 21:06:15:841_0
- RFN: 189
- Chip: 18944
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB2 LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 1
. . . . . . . (BitStringType)sib_Data_variable[-1] = "1100010000000000000001011000100000101000000010100001000111100000000101000000000000000000000011000111010000"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 2
. . . . . . . (BitStringType)sib_Data_variable[-1] = "10000000000000000001"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 1c 02 01 00 02 01 ff 00 0e 21 69 c4 00 05 88 28 0a 11 e0 14 00 00 0c 74 04 27 00 00 20

- No.: 406
- Timestamp: 21:06:15:851_0
- RFN: 190
- Chip: 18176
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 10
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 0a

- No.: 411
- Timestamp: 21:06:15:856_0
- RFN: 190
- Chip: 36608
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB3 LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 412
- Timestamp: 21:06:15:861_0
- RFN: 191
- Chip: 17664
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB3 LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 7
. . . . . . . (BitStringType)sib_Data_variable[-1] = "101000101000000010000001"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 3
. . . . . . . (BitStringType)sib_Data_variable[-1] = "110000000000000000000000000000000100000011001100011000000000100100001000000100011111111111111111111111"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 1c 02 01 00 02 01 ff 00 0e 27 17 a2 80 81 1b 2e 00 00 00 02 06 63 00 48 40 8f ff ff e0

- No.: 424
- Timestamp: 21:06:15:871_0
- RFN: 192
- Chip: 18944
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 26
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 1a

- No.: 429
- Timestamp: 21:06:15:876_0
- RFN: 192
- Chip: 36864
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB4 LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 430
- Timestamp: 21:06:15:881_0
- RFN: 193
- Chip: 18176
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB4 LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 7
. . . . . . . (BitStringType)sib_Data_variable[-1] = "101000101000000010000001"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 4
. . . . . . . (BitStringType)sib_Data_variable[-1] = "1000000000000000000000000000000101100110001100000000010010000100000010001110111"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 19 02 01 00 02 01 ff 00 0e 27 17 a2 80 81 22 74 00 00 00 0b 31 80 24 20 47 70

- No.: 447
- Timestamp: 21:06:15:928_0
- RFN: 198
- Chip: 8448
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 23
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 17

- No.: 452
- Timestamp: 21:06:15:934_0
- RFN: 198
- Chip: 32000
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB5 LINE 41
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 453
- Timestamp: 21:06:15:938_0
- RFN: 199
- Chip: 8448
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB5 LINE 42
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 08 02 01 00 02 01 ff 00 00

- No.: 457
- Timestamp: 21:06:15:942_0
- RFN: 199
- Chip: 23552
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 19
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 13

- No.: 462
- Timestamp: 21:06:15:954_0
- RFN: 200
- Chip: 32768
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB5 LINE 44
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 463
- Timestamp: 21:06:15:959_0
- RFN: 201
- Chip: 11776
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB5 LINE 45
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . FirstSegment
. . . . . . (SIB_Type)sib_Type = 5
. . . . . . (IntegerType)seg_Count = 3
. . . . . . (BitStringType)sib_Data_fixed[222] = "001101010100010000111110000000001111111101000011111111111111110111010010000100001111000000101001000011000000101010100101010110000000000000001100110001011011010101111110001010111010000011111110100000111111101000001111111010"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 25 02 01 00 02 01 ff 00 02 52 35 44 3e 00 ff 43 ff fd d2 10 f0 29 0c 0a a5 58 00 0c c5 b5 7e 2b a0 fe 83 fa 0f e8

- No.: 467
- Timestamp: 21:06:15:964_0
- RFN: 201
- Chip: 30208
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 21
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 15

- No.: 472
- Timestamp: 21:06:15:974_0
- RFN: 202
- Chip: 33792
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB5 LINE 47
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 473
- Timestamp: 21:06:15:979_0
- RFN: 203
- Chip: 13568
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB5 LINE 48
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . SubsequentSegment
. . . . . . (SIB_Type)sib_Type = 5
. . . . . . (IntegerType)segmentIndex = 1
. . . . . . (BitStringType)sib_Data_fixed[222] = "000011111111010000000000000000001101011000110100010000111111010011100101000001100001000011001010000000110000001110001001000000010110000000000000100000001110000000001000100001100100001010011001000010100000000000110000000100"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 25 02 01 00 02 01 ff 00 04 50 0f f4 00 00 d6 34 43 f4 e5 06 10 ca 03 03 89 01 60 00 80 e0 08 86 42 99 0a 00 30 10

- No.: 477
- Timestamp: 21:06:15:983_0
- RFN: 203
- Chip: 29696
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 22
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 16

- No.: 482
- Timestamp: 21:06:15:994_0
- RFN: 204
- Chip: 32768
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB5 LINE 50
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 484
- Timestamp: 21:06:15:999_0
- RFN: 205
- Chip: 13824
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB5 LINE 52
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . LastSegmentShort
. . . . . . (SIB_Type)sib_Type = 5
. . . . . . (IntegerType)segmentIndex = 2
. . . . . . (BitStringType)sib_Data_variable[-1] = "010001011100101011010110100000000000011110001000011000000001011011011011011000100000000001000011000010001001010000001011011010000000010000"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 1c 02 01 00 02 01 ff 00 06 51 89 45 ca d6 80 07 88 60 16 db 62 00 43 08 94 0b 68 04 00

- No.: 501
- Timestamp: 21:06:16:010_0
- RFN: 206
- Chip: 18176
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 3
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 03

- No.: 506
- Timestamp: 21:06:16:015_0
- RFN: 206
- Chip: 36352
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB6 LINE 8
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 509
- Timestamp: 21:06:16:020_0
- RFN: 207
- Chip: 17920
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB6:lt_CompleteSIB LINE 4
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 6
. . . . . . . (BitStringType)sib_Data_variable[-1] = "0000001010010001"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 0c 02 01 00 02 01 ff 00 0e 06 0f 02 91

- No.: 514
- Timestamp: 21:06:16:024_0
- RFN: 207
- Chip: 34560
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 5
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 05

- No.: 519
- Timestamp: 21:06:16:034_0
- RFN: 208
- Chip: 34048
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB6 LINE 11
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 520
- Timestamp: 21:06:16:038_0
- RFN: 209
- Chip: 10752
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB6 LINE 12
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 08 02 01 00 02 01 ff 00 00

- No.: 524
- Timestamp: 21:06:16:042_0
- RFN: 209
- Chip: 24832
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 6
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 06

- No.: 529
- Timestamp: 21:06:16:054_0
- RFN: 210
- Chip: 33024
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB6 LINE 14
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 530
- Timestamp: 21:06:16:058_0
- RFN: 211
- Chip: 11008
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB6 LINE 15
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 08 02 01 00 02 01 ff 00 00

- No.: 534
- Timestamp: 21:06:16:062_0
- RFN: 211
- Chip: 26112
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 7
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 07

- No.: 539
- Timestamp: 21:06:16:074_0
- RFN: 212
- Chip: 32768
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB6 LINE 17
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 540
- Timestamp: 21:06:16:078_0
- RFN: 213
- Chip: 9216
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB6 LINE 18
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 08 02 01 00 02 01 ff 00 00

- No.: 548
- Timestamp: 21:06:16:091_0
- RFN: 214
- Chip: 23296
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 2
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 02

- No.: 553
- Timestamp: 21:06:16:100_0
- RFN: 215
- Chip: 13056
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB7 LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 556
- Timestamp: 21:06:16:108_0
- RFN: 216
- Chip: 5120
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB7:lt_CompleteSIB LINE 4
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 7
. . . . . . . (BitStringType)sib_Data_variable[-1] = "101000101000000010000001"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 0d 02 01 00 02 01 ff 00 0e 07 17 a2 80 81

- No.: 564
- Timestamp: 21:06:16:123_0
- RFN: 217
- Chip: 24576
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 10
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 0a

- No.: 569
- Timestamp: 21:06:16:135_0
- RFN: 218
- Chip: 34816
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB7:lt_ConcatWithSIB3 LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 570
- Timestamp: 21:06:16:142_0
- RFN: 219
- Chip: 21760
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB7:lt_ConcatWithSIB3 LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 7
. . . . . . . (BitStringType)sib_Data_variable[-1] = "101000101000000010000001"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 3
. . . . . . . (BitStringType)sib_Data_variable[-1] = "110000000000000000000000000000000100000011001100011000000000100100001000000100011111111111111111111111"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 1c 02 01 00 02 01 ff 00 0e 27 17 a2 80 81 1b 2e 00 00 00 02 06 63 00 48 40 8f ff ff e0

- No.: 578
- Timestamp: 21:06:16:156_0
- RFN: 220
- Chip: 36864
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 18
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 12

- No.: 583
- Timestamp: 21:06:16:165_0
- RFN: 221
- Chip: 35840
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB7:lt_ConcatWithSIB18 LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 584
- Timestamp: 21:06:16:172_0
- RFN: 222
- Chip: 21760
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB7:lt_ConcatWithSIB18 LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 7
. . . . . . . (BitStringType)sib_Data_variable[-1] = "101000101000000010000001"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 26
. . . . . . . (BitStringType)sib_Data_variable[-1] = "100100000001000000000001000000001"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 13 02 01 00 02 01 ff 00 0e 27 17 a2 80 81 d1 04 80 80 08 04

- No.: 592
- Timestamp: 21:06:16:186_0
- RFN: 223
- Chip: 38144
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 26
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 1a

- No.: 597
- Timestamp: 21:06:16:196_0
- RFN: 224
- Chip: 37120
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB7:lt_ConcatWithSIB4 LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 598
- Timestamp: 21:06:16:202_0
- RFN: 225
- Chip: 23808
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB7:lt_ConcatWithSIB4 LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 7
. . . . . . . (BitStringType)sib_Data_variable[-1] = "101000101000000010000001"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 4
. . . . . . . (BitStringType)sib_Data_variable[-1] = "1000000000000000000000000000000101100110001100000000010010000100000010001110111"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 19 02 01 00 02 01 ff 00 0e 27 17 a2 80 81 22 74 00 00 00 0b 31 80 24 20 47 70

- No.: 612
- Timestamp: 21:06:16:214_0
- RFN: 226
- Chip: 29952
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 31
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 1f

- No.: 617
- Timestamp: 21:06:16:218_0
- RFN: 227
- Chip: 9216
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB11 LINE 20
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 618
- Timestamp: 21:06:16:222_0
- RFN: 227
- Chip: 23808
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB11 LINE 21
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 08 02 01 00 02 01 ff 00 00

- No.: 622
- Timestamp: 21:06:16:226_0
- RFN: 228
- Chip: 0
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 29
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 1d

- No.: 627
- Timestamp: 21:06:16:235_0
- RFN: 228
- Chip: 36352
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB11 LINE 23
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 628
- Timestamp: 21:06:16:240_0
- RFN: 229
- Chip: 15360
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB11 LINE 24
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . FirstSegment
. . . . . . (SIB_Type)sib_Type = 11
. . . . . . (IntegerType)seg_Count = 2
. . . . . . (BitStringType)sib_Data_fixed[222] = "011000001101100100010010000000001000110010000100001000010010010110101000100000100110010001010011000001011001000010100111000010111000010100001000100010001100100101010100000001001010000101001010100001100001001010001000001010"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 25 02 01 00 02 01 ff 00 02 b1 60 d9 12 00 8c 84 21 25 a8 82 64 53 05 90 a7 0b 85 08 88 c9 54 04 a1 4a 86 12 88 28

- No.: 632
- Timestamp: 21:06:16:244_0
- RFN: 229
- Chip: 33280
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 30
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 1e

- No.: 637
- Timestamp: 21:06:16:254_0
- RFN: 230
- Chip: 33280
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB11 LINE 26
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 639
- Timestamp: 21:06:16:260_0
- RFN: 231
- Chip: 14848
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB11 LINE 28
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . LastSegmentShort
. . . . . . (SIB_Type)sib_Type = 11
. . . . . . (IntegerType)segmentIndex = 1
. . . . . . (BitStringType)sib_Data_variable[-1] = "000100001100001001010010011010101000011000010010101000101100011001010100101010100001001111101000100010000001010010110000100010100001010101111000"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 1c 02 01 00 02 01 ff 00 06 b0 8f 10 c2 52 6a 86 12 a2 c6 54 aa 13 e8 88 14 b0 8a 15 78

- No.: 652
- Timestamp: 21:06:16:269_0
- RFN: 232
- Chip: 12544
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 13
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 0d

- No.: 657
- Timestamp: 21:06:16:275_0
- RFN: 232
- Chip: 36608
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB12 LINE 8
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 660
- Timestamp: 21:06:16:281_0
- RFN: 233
- Chip: 18688
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB12:lt_CompleteSIB LINE 4
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 12
. . . . . . . (BitStringType)sib_Data_variable[-1] = "010000000"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 0c 02 01 00 02 01 ff 00 0e 0c 08 40 00

- No.: 665
- Timestamp: 21:06:16:285_0
- RFN: 233
- Chip: 35072
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 14
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 0e

- No.: 670
- Timestamp: 21:06:16:294_0
- RFN: 234
- Chip: 33024
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB12 LINE 11
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 671
- Timestamp: 21:06:16:298_0
- RFN: 235
- Chip: 9984
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB12 LINE 12
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 08 02 01 00 02 01 ff 00 00

- No.: 675
- Timestamp: 21:06:16:302_0
- RFN: 235
- Chip: 25344
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 15
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 0f

- No.: 680
- Timestamp: 21:06:16:314_0
- RFN: 236
- Chip: 33792
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB12 LINE 14
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 681
- Timestamp: 21:06:16:318_0
- RFN: 237
- Chip: 10496
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB12 LINE 15
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 08 02 01 00 02 01 ff 00 00

- No.: 689
- Timestamp: 21:06:16:326_0
- RFN: 238
- Chip: 1792
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 18
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 12

- No.: 694
- Timestamp: 21:06:16:335_0
- RFN: 238
- Chip: 36864
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB18 LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 695
- Timestamp: 21:06:16:340_0
- RFN: 239
- Chip: 18176
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB18 LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 7
. . . . . . . (BitStringType)sib_Data_variable[-1] = "101000101000000010000001"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 26
. . . . . . . (BitStringType)sib_Data_variable[-1] = "100100000001000000000001000000001"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 13 02 01 00 02 01 ff 00 0e 27 17 a2 80 81 d1 04 80 80 08 04

- No.: 707
- Timestamp: 21:06:16:349_0
- RFN: 240
- Chip: 12544
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 4
. . (IntegerType)sg_POS = 1
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 04 02 01 01

- No.: 712
- Timestamp: 21:06:16:355_0
- RFN: 240
- Chip: 37376
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSB1_DefSchedul LINE 4
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 715
- Timestamp: 21:06:16:361_0
- RFN: 241
- Chip: 19968
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSB1_DefSchedul:lt_CompleteSIB LINE 4
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 27
. . . . . . . (BitStringType)sib_Data_variable[-1] = "10010000101010001000001100110000010010010100111000101001110100000000010110100010001101110010100010010010"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 17 02 01 00 02 01 ff 00 0e 1b 67 90 a8 83 30 49 4e 29 d0 05 a2 37 28 92

- No.: 733
- Timestamp: 21:06:16:372_0
- RFN: 242
- Chip: 25088
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 3
. . (IntegerType)sg_POS = 0
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 03 02 01 00

- No.: 738
- Timestamp: 21:06:16:376_0
- RFN: 243
- Chip: 3840
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendMIB LINE 7
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 741
- Timestamp: 21:06:16:382_0
- RFN: 243
- Chip: 25088
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendMIB:lt_CompleteSIB LINE 4
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 0
. . . . . . . (BitStringType)sib_Data_variable[-1] = "0001000000000000010000000010010110101010000100010000000000001000100010110000101000100010110001001000100010100001101000100110100010001110010010010011000100010000"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 1e 02 01 00 02 01 ff 00 0e 00 9f 10 00 40 25 aa 11 00 08 8b 0a 22 c4 88 a1 a2 68 8e 49 31 10

- No.: 756
- Timestamp: 21:06:16:388_0
- RFN: 244
- Chip: 11264
- Event: Send
- PCO: Ut
- Message: MMI_CmdReq
- Source: ts_MMI_UE_SwitchOn LINE 1
- Message Structure:
MMI_CmdReq
. (IA5StringType)cmd[-1] = "Please switch on the UE"
- Constraint:
ca_MMI_CmdReq
- BinaryMessage:
50 6c 65 61 73 65 20 73 77 69 74 63 68 20 6f 6e 20 74 68 65 20 55 45

- No.: 763
- Timestamp: 21:06:24:717_0
- RFN: 1077
- Chip: 3072
- Event: Receive
- PCO: Ut
- Message: MMI_CmdCnf
- Source: ts_MMI_UE_SwitchOn LINE 2
- Message Structure:
MMI_CmdCnf
. (BooleanType)result = TRUE
. (IA5StringType)resultString[6] = " OK "
- Constraint:
ca_MMI_CmdCnf
- BinaryMessage:
80 0d 0a 4f 4b 0d 0a

- No.: 779
- Timestamp: 21:06:24:726_0
- RFN: 1078
- Chip: 2816
- Event: Receive
- PCO: TM
- Message: RLC_TR_DATA_IND
- Source: ts_RRC_ConnEst:lt_RcvConnReq LINE 2
- Message Structure:
RLC_TR_DATA_IND
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
. tM_message
. . UL_CCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode = 0
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . UL_CCCH_MessageType
. . . . RRCConnectionRequest
. . . . . InitialUE_Identity
. . . . . . TMSI_and_LAI_GSM_MAP
. . . . . . . (BitStringType)tmsi[32] = "00010010001101000101011001111000"
. . . . . . . LAI
. . . . . . . . PLMN_Identity
. . . . . . . . . MCC
. . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . (IntegerType)_elem = 1
. . . . . . . . . MNC
. . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . (IntegerType)_elem = 1
. . . . . . . . (BitStringType)lac[16] = '0000000000000001'B
. . . . . (EstablishmentCause)establishmentCause = 12
. . . . . (ProtocolErrorIndicator)protocolErrorIndicator = 0
. . . . . MeasuredResultsOnRACH
. . . . . . currentCell
. . . . . . . modeSpecificInfo
. . . . . . . . fdd
. . . . . . . . . measurementQuantity
. . . . . . . . . . (IntegerType)cpich_Ec_N0 = 0
. . . . . v3d0NonCriticalExtensions
. . . . . . RRCConnectionRequest_v3d0ext_IEs
. . . . . . . (BitStringType)uESpecificBehaviourInformation1idle = 0
. . . . . . nonCriticalExtensions
- Constraint:
car_RRC_ConnReq
- BinaryMessage:
30 11 02 01 00 02 01 00 21 12 34 56 78 00 10 08 00 0b 00

- No.: 783
- Timestamp: 21:06:24:787_0
- RFN: 1084
- Chip: 5888
- Event: Send
- PCO: UM
- Message: RLC_UM_DATA_REQ
- Source: ts_RRC_ConnEst:lt_Send_ConnSetUp LINE 22
- Message Structure:
RLC_UM_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
. uM_message
. . DL_CCCH_Message
. . . IntegrityCheckInfo
. . . DL_CCCH_MessageType
. . . . RRCConnectionSetup
. . . . . r3
. . . . . . RRCConnectionSetup_r3_IEs
. . . . . . . InitialUE_Identity
. . . . . . . . TMSI_and_LAI_GSM_MAP
. . . . . . . . . (BitStringType)tmsi[32] = "00010010001101000101011001111000"
. . . . . . . . . LAI
. . . . . . . . . . PLMN_Identity
. . . . . . . . . . . MCC
. . . . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . . . (IntegerType)_elem = 1
. . . . . . . . . . . MNC
. . . . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . . . (IntegerType)_elem = 1
. . . . . . . . . . (BitStringType)lac[16] = '0000000000000001'B
. . . . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . . . (IntegerType)activationTime = -
. . . . . . . U_RNTI
. . . . . . . . (BitStringType)srnc_Identity[12] = "000000000001"
. . . . . . . . (BitStringType)s_RNTI[20] = "00000000000000000001"
. . . . . . . (BitStringType)new_c_RNTI[16] = -
. . . . . . . (RRC_StateIndicator)rrc_StateIndicator = 0
. . . . . . . (IntegerType)utran_DRX_CycleLengthCoeff = 9
. . . . . . . CapabilityUpdateRequirement
. . . . . . . . (BooleanType)ue_RadioCapabilityFDDUpdateRequirement = TRUE
. . . . . . . . (BooleanType)ue_RadioCapabilityTDDUpdateRequirement = FALSE
. . . . . . . . SystemSpecificCapUpdateReqList
. . . . . . . . . (SystemSpecificCapUpdateReq)_elem = 0
. . . . . . . SRB_InformationSetupList2
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_UM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 1
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 1
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . . . . . . . (TimerRST)timerRST = 9
. . . . . . . . . . . . . (MaxRST)max_RST = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 2
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 2
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . . . . . . . (TimerRST)timerRST = 9
. . . . . . . . . . . . . (MaxRST)max_RST = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 3
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 3
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . . . . . . . (TimerRST)timerRST = 9
. . . . . . . . . . . . . (MaxRST)max_RST = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 4
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 4
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . UL_CommonTransChInfo
. . . . . . . . TFC_Subset
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . TFCS
. . . . . . . . . . . ExplicitTFCS_Configuration
. . . . . . . . . . . . TFCS_ReconfAdd
. . . . . . . . . . . . . ctfcSize
. . . . . . . . . . . . . . ctfc2Bit
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . . . . . . . (IntegerType)ctfc2 = 0
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . . . . . . . (IntegerType)ctfc2 = 1
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 11
. . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . UL_AddReconfTransChInfoList
. . . . . . . . UL_AddReconfTransChInformation
. . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType = 0
. . . . . . . . . (IntegerType)transportChannelIdentity = 5
. . . . . . . . . TransportFormatSet
. . . . . . . . . . DedicatedTransChTFS
. . . . . . . . . . . tti
. . . . . . . . . . . . DedicatedDynamicTF_InfoList
. . . . . . . . . . . . . DedicatedDynamicTF_Info
. . . . . . . . . . . . . . rlc_Size
. . . . . . . . . . . . . . . BitModeRLC_SizeInfo
. . . . . . . . . . . . . . . . sizeType2
. . . . . . . . . . . . . . . . . (IntegerType)part1 = 2
. . . . . . . . . . . . . . . . . (IntegerType)part2 = -
. . . . . . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . LogicalChannelList
. . . . . . . . . . . SemistaticTF_Information
. . . . . . . . . . . . ChannelCodingType
. . . . . . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . . . . . (IntegerType)rateMatchingAttribute = 192
. . . . . . . . . . . . (CRC_Size)crc_Size = 3
. . . . . . . DL_CommonTransChInfo
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . dl_Parameters
. . . . . . . DL_AddReconfTransChInfoList
. . . . . . . . DL_AddReconfTransChInformation
. . . . . . . . . (DL_TrCH_Type)dl_TransportChannelType = 0
. . . . . . . . . (IntegerType)dl_transportChannelIdentity = 10
. . . . . . . . . tfs_SignallingMode
. . . . . . . . . . UL_TransportChannelIdentity
. . . . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType = 0
. . . . . . . . . . . (IntegerType)ul_TransportChannelIdentity = 5
. . . . . . . . . QualityTarget
. . . . . . . . . . (IntegerType)bler_QualityValue = -20
. . . . . . . . . TM_SignallingInfo
. . . . . . . FrequencyInfo
. . . . . . . (IntegerType)maxAllowedUL_TX_Power = -
. . . . . . . UL_ChannelRequirement
. . . . . . . . UL_DPCH_Info
. . . . . . . . . UL_DPCH_PowerControlInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (IntegerType)dpcch_PowerOffset = -40
. . . . . . . . . . . (IntegerType)pc_Preamble = 1
. . . . . . . . . . . (IntegerType)sRB_delay = 7
. . . . . . . . . . . PowerControlAlgorithm
. . . . . . . . . . . . (IntegerType)algorithm1 = 1
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (ScramblingCodeType)scramblingCodeType = 1
. . . . . . . . . . . (IntegerType)scramblingCode = 0
. . . . . . . . . . . (IntegerType)numberOfDPDCH = -
. . . . . . . . . . . (SpreadingFactor)spreadingFactor = 4
. . . . . . . . . . . (BooleanType)tfci_Existence = TRUE
. . . . . . . . . . . (IntegerType)numberOfFBI_Bits = -
. . . . . . . . . . . (PuncturingLimit)puncturingLimit = 15
. . . . . . . DL_CommonInformation
. . . . . . . . DL_DPCH_InfoCommon
. . . . . . . . . cfnHandling
. . . . . . . . . . initialise
. . . . . . . . . . . (IntegerType)cfntargetsfnframeoffset = -
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . DL_DPCH_PowerControlInfo
. . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . (DPC_Mode)dpc_Mode = 0
. . . . . . . . . . . (IntegerType)powerOffsetPilot_pdpdch = 0
. . . . . . . . . . . Dl_rate_matching_restriction
. . . . . . . . . . . SF512_AndPilot
. . . . . . . . . . . . (PilotBits128)sfd128 = 0
. . . . . . . . . . . (PositionFixedOrFlexible)positionFixedOrFlexible = 0
. . . . . . . . . . . (BooleanType)tfci_Existence = FALSE
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . (IntegerType)defaultDPCH_OffsetValue = 0
. . . . . . . . . . DPCH_CompressedModeInfo
. . . . . . . . . . (TX_DiversityMode)tx_DiversityMode = 0
. . . . . . . . . . SSDT_Information
. . . . . . . DL_InformationPerRL_List
. . . . . . . . DL_InformationPerRL
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . PrimaryCPICH_Info
. . . . . . . . . . . . (IntegerType)primaryScramblingCode = 100
. . . . . . . . . . . PDSCH_SHO_DCH_Info
. . . . . . . . . . . PDSCH_CodeMapping
. . . . . . . . . DL_DPCH_InfoPerRL
. . . . . . . . . . fdd
. . . . . . . . . . . (PCPICH_UsageForChannelEst)pCPICH_UsageForChannelEst = 0
. . . . . . . . . . . (IntegerType)dpch_FrameOffset = 0
. . . . . . . . . . . SecondaryCPICH_Info
. . . . . . . . . . . DL_ChannelisationCodeList
. . . . . . . . . . . . DL_ChannelisationCode
. . . . . . . . . . . . . (IntegerType)secondaryScramblingCode = 1
. . . . . . . . . . . . . SF512_AndCodeNumber
. . . . . . . . . . . . . . (IntegerType)sf128 = 0
. . . . . . . . . . . . . (ScramblingCodeChange)scramblingCodeChange = 1
. . . . . . . . . . . (IntegerType)tpc_CombinationIndex = 0
. . . . . . . . . . . (SSDT_CellIdentity)ssdt_CellIdentity = -
. . . . . . . . . . . (ClosedLoopTimingAdjMode)closedLoopTimingAdjMode = -
. . . . . . . . . SCCPCH_InfoForFACH
. . . . . . laterNonCriticalExtensions
. (BooleanType)specialLI = TRUE
- Constraint:
cas_RRC_ConnSetup
- BinaryMessage:
30 78 02 01 00 02 01 00 30 e7 22 46 8a cf 00 02 01 00 01 00 04 00 00 4d 82 69 3a 10 10 89 0d 42 00 02 81 9e 8e 46 c9 ce 7c 9c 4e 74 20 a5 12 3a 8c 00 15 13 3d 1c 8d 93 9c f9 38 9c e8 42 52 24 b5 28 00 4a 46 7a 39 1b 27 39 f2 71 39 d0 86 b4 49 ea 70 00 d4 c8 00 06 25 2b f0 02 00 08 82 23 bf 66 08 98 95 a5 47 a2 00 00 01 3f 90 0a 14 00 02 06 40 00 0c 28 08 01 01 ff

- No.: 804
- Timestamp: 21:06:24:831_0
- RFN: 1088
- Chip: 20736
- Event: Start Timer
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 3
- Message Structure:
no details available
- Constraint:
t_WaitMS (13500 Ms)
- BinaryMessage:

- No.: 809
- Timestamp: 21:06:25:044_0
- RFN: 1109
- Chip: 31744
- Event: Receive
- PCO: CPHY
- Message: CPHY_Sync_IND
- Source: RRC_Def1 LINE 13
- Message Structure:
CPHY_Sync_IND
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_SyncInd
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 810
- Timestamp: 21:06:25:044_1
- RFN: 1109
- Chip: 33280
- Event: Cancel Timer
- Source: RRC_Def1 LINE 13
- Message Structure:
no details available
- Constraint:
t_T312
- BinaryMessage:

- No.: 811
- Timestamp: 21:06:25:045_0
- RFN: 1109
- Chip: 35328
- Event: Default
- Source: RRC_Def1 LINE 0
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 812
- Timestamp: 21:06:25:045_1
- RFN: 1109
- Chip: 36096
- Event: Default
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 817
- Timestamp: 21:06:25:159_0
- RFN: 1121
- Chip: 13312
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_IND
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
RLC_AM_DATA_IND
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. IntegrityResult
. . (IntegrityStatus)integrityUsed = 0
. aM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode = 0
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . UL_DCCH_MessageType
. . . . RRCConnectionSetupComplete
. . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . STARTList
. . . . . . STARTSingle
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity = 1
. . . . . . . (BitStringType)start_Value[20] = "00000000000000000100"
. . . . . . STARTSingle
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity = 0
. . . . . . . (BitStringType)start_Value[20] = "00000000000000000010"
. . . . . UE_RadioAccessCapability
. . . . . . (AccessStratumReleaseIndicator)accessStratumReleaseIndicator = 0
. . . . . . PDCP_Capability
. . . . . . . (BooleanType)losslessSRNS_RelocationSupport = FALSE
. . . . . . . supportForRfc2507
. . . . . . RLC_Capability
. . . . . . . (TotalRLC_AM_BufferSize)totalRLC_AM_BufferSize = 2
. . . . . . . (MaximumRLC_WindowSize)maximumRLC_WindowSize = 0
. . . . . . . (MaximumAM_EntityNumberRLC_Cap)maximumAM_EntityNumber = 3
. . . . . . TransportChannelCapability
. . . . . . . DL_TransChCapability
. . . . . . . . (MaxNoBits)maxNoBitsReceived = 4
. . . . . . . . (MaxNoBits)maxConvCodeBitsReceived = 1
. . . . . . . . TurboSupport
. . . . . . . . . (MaxNoBits)supported = 4
. . . . . . . . (MaxSimultaneousTransChsDL)maxSimultaneousTransChs = 1
. . . . . . . . (IntegerType)maxSimultaneousCCTrCH_Count = 1
. . . . . . . . (MaxTransportBlocksDL)maxReceivedTransportBlocks = 2
. . . . . . . . (MaxNumberOfTFC_DL)maxNumberOfTFC = 4
. . . . . . . . (MaxNumberOfTF)maxNumberOfTF = 1
. . . . . . . UL_TransChCapability
. . . . . . . . (MaxNoBits)maxNoBitsTransmitted = 3
. . . . . . . . (MaxNoBits)maxConvCodeBitsTransmitted = 1
. . . . . . . . TurboSupport
. . . . . . . . . (MaxNoBits)supported = 3
. . . . . . . . (MaxSimultaneousTransChsUL)maxSimultaneousTransChs = 2
. . . . . . . . modeSpecificInfo
. . . . . . . . (MaxTransportBlocksUL)maxTransmittedBlocks = 2
. . . . . . . . (MaxNumberOfTFC_UL)maxNumberOfTFC = 3
. . . . . . . . (MaxNumberOfTF)maxNumberOfTF = 0
. . . . . . RF_Capability
. . . . . . . fddRF_Capability
. . . . . . . . (IntegerType)ue_PowerClass = 4
. . . . . . . . (TxRxFrequencySeparation)txRxFrequencySeparation = 0
. . . . . . . tddRF_Capability
. . . . . . . . (IntegerType)ue_PowerClass = 0
. . . . . . . . (RadioFrequencyBandTDDList)radioFrequencyTDDBandList = 0
. . . . . . . . (ChipRateCapability)chipRateCapability = 0
. . . . . . PhysicalChannelCapability
. . . . . . . fddPhysChCapability
. . . . . . . . DL_PhysChCapabilityFDD
. . . . . . . . . (IntegerType)maxNoDPCH_PDSCH_Codes = 3
. . . . . . . . . (MaxNoPhysChBitsReceived)maxNoPhysChBitsReceived = 6
. . . . . . . . . (BooleanType)supportForSF_512 = FALSE
. . . . . . . . . (BooleanType)supportOfPDSCH = FALSE
. . . . . . . . . SimultaneousSCCPCH_DPCH_Reception
. . . . . . . . UL_PhysChCapabilityFDD
. . . . . . . . . (MaxNoDPDCH_BitsTransmitted)maxNoDPDCH_BitsTransmitted = 2
. . . . . . . . . (BooleanType)supportOfPCPCH = FALSE
. . . . . . . tddPhysChCapability
. . . . . . . . DL_PhysChCapabilityTDD
. . . . . . . . . (IntegerType)maxTS_PerFrame = 0
. . . . . . . . . (IntegerType)maxPhysChPerFrame = 0
. . . . . . . . . (MinimumSF_DL)minimumSF = 0
. . . . . . . . . (BooleanType)supportOfPDSCH = FALSE
. . . . . . . . . (IntegerType)maxPhysChPerTS = 0
. . . . . . . . UL_PhysChCapabilityTDD
. . . . . . . . . (IntegerType)maxTS_PerFrame = 0
. . . . . . . . . (MaxPhysChPerTimeslot)maxPhysChPerTimeslot = 0
. . . . . . . . . (MinimumSF_UL)minimumSF = 0
. . . . . . . . . (BooleanType)supportOfPUSCH = FALSE
. . . . . . UE_MultiModeRAT_Capability
. . . . . . . MultiRAT_Capability
. . . . . . . . (BooleanType)supportOfGSM = TRUE
. . . . . . . . (BooleanType)supportOfMulticarrier = FALSE
. . . . . . . (MultiModeCapability)multiModeCapability = 1
. . . . . . SecurityCapability
. . . . . . . (BitStringType)cipheringAlgorithmCap[16] = '0000000000000011'B
. . . . . . . (BitStringType)integrityProtectionAlgorithmCap[16] = '0000000000000010'B
. . . . . . UE_Positioning_Capability
. . . . . . . (BooleanType)standaloneLocMethodsSupported = FALSE
. . . . . . . (BooleanType)ue_BasedOTDOA_Supported = FALSE
. . . . . . . (NetworkAssistedGPS_Supported)networkAssistedGPS_Supported = 3
. . . . . . . (BooleanType)supportForUE_GPS_TimingOfCellFrames = FALSE
. . . . . . . (BooleanType)supportForIPDL = FALSE
. . . . . . MeasurementCapability
. . . . . . . CompressedModeMeasCapability
. . . . . . . . (BooleanType)fdd_Measurements = TRUE
. . . . . . . . (BooleanType)tdd_Measurements = FALSE
. . . . . . . . GSM_Measurements
. . . . . . . . . (BooleanType)gsm900 = TRUE
. . . . . . . . . (BooleanType)dcs1800 = TRUE
. . . . . . . . . (BooleanType)gsm1900 = FALSE
. . . . . . . . (BooleanType)multiCarrierMeasurements = FALSE
. . . . . . . CompressedModeMeasCapability
. . . . . . . . (BooleanType)fdd_Measurements = TRUE
. . . . . . . . (BooleanType)tdd_Measurements = FALSE
. . . . . . . . GSM_Measurements
. . . . . . . . . (BooleanType)gsm900 = TRUE
. . . . . . . . . (BooleanType)dcs1800 = TRUE
. . . . . . . . . (BooleanType)gsm1900 = FALSE
. . . . . . . . (BooleanType)multiCarrierMeasurements = FALSE
. . . . . v370NonCriticalExtensions
. . . . . . RRCConnectionSetupComplete_v370ext
. . . . . . . UE_RadioAccessCapability_v370ext
. . . . . . v380NonCriticalExtensions
. . . . . . . RRCConnectionSetupComplete_v380ext_IEs
. . . . . . . . UE_RadioAccessCapability_v380ext
. . . . . . . . . UE_PositioningCapabilityExt_v380
. . . . . . . . . . (BooleanType)rx_tx_TimeDifferenceType2Capable = FALSE
. . . . . . . . DL_PhysChCapabilityFDD_v380ext
. . . . . . . . . (SupportOfDedicatedPilotsForChEstimation)supportOfDedicatedPilotsForChEstimation = 0
. . . . . . . v3a0NonCriticalExtensions
. . . . . . . . RRCConnectionSetupComplete_v3a0ext_IEs
. . . . . . . . . UE_RadioAccessCapability_v3a0ext
. . . . . . . . . . UE_PositioningCapabilityExt_v3a0
. . . . . . . . . . . (UE_PositioningCapabilityExt_v3a0_list_0)validity_CellPCH_UraPCH = 0
. . . . . . . . laterNonCriticalExtensions
. . . . . . . . . (BitStringType)rrcConnectionSetupComplete_r3_add_ext = 0
. . . . . . . . . nonCriticalExtensions
- Constraint:
car_RRC_ConnSetupCmpl
- BinaryMessage:
30 27 02 01 ff 02 01 02 0a 05 01 00 00 00 00 4a 0c 00 01 00 00 05 11 a0 d1 04 84 c6 68 46 2c 93 02 48 00 18 00 11 8f 8f 80

- No.: 818
- Timestamp: 21:06:25:170_0
- RFN: 1122
- Chip: 16640
- Event: Cancel Timer
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
t_WaitMS
- BinaryMessage:

- No.: 819
- Timestamp: 21:06:25:170_1
- RFN: 1122
- Chip: 17408
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 833
- Timestamp: 21:06:25:176_0
- RFN: 1123
- Chip: 2560
- Event: Send
- PCO: CMAC
- Message: CMAC_SecurityMode_Config_REQ
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 1
- Message Structure:
CMAC_SecurityMode_Config_REQ
. (IntegerType)cellId = 0
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity = 1
. . (BitStringType)startValue[20] = "00000000000000000100"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = -
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CMAC_SecurityModeCfgReq
- BinaryMessage:
30 0e 02 01 00 30 09 0a 01 01 03 04 04 00 00 40

- No.: 834
- Timestamp: 21:06:25:178_0
- RFN: 1123
- Chip: 9472
- Event: Receive
- PCO: CMAC
- Message: CMAC_SecurityMode_Config_CNF
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 2
- Message Structure:
CMAC_SecurityMode_Config_CNF
. (IntegerType)cellId = 0
- Constraint:
ca_CMAC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 00

- No.: 835
- Timestamp: 21:06:25:180_0
- RFN: 1123
- Chip: 16640
- Event: Send
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_REQ
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 3
- Message Structure:
CRLC_SecurityMode_Config_REQ
. (IntegerType)cellId = -1
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity = 1
. . (BitStringType)startValue[20] = "00000000000000000100"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = -
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CRLC_SecurityModeCfgReq
- BinaryMessage:
30 0e 02 01 ff 30 09 0a 01 01 03 04 04 00 00 40

- No.: 836
- Timestamp: 21:06:25:181_0
- RFN: 1123
- Chip: 22784
- Event: Receive
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_CNF
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 4
- Message Structure:
CRLC_SecurityMode_Config_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 850
- Timestamp: 21:06:25:187_0
- RFN: 1124
- Chip: 3840
- Event: Send
- PCO: CMAC
- Message: CMAC_SecurityMode_Config_REQ
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 1
- Message Structure:
CMAC_SecurityMode_Config_REQ
. (IntegerType)cellId = 0
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity = 0
. . (BitStringType)startValue[20] = "00000000000000000010"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = -
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CMAC_SecurityModeCfgReq
- BinaryMessage:
30 0e 02 01 00 30 09 0a 01 00 03 04 04 00 00 20

- No.: 851
- Timestamp: 21:06:25:189_0
- RFN: 1124
- Chip: 10240
- Event: Receive
- PCO: CMAC
- Message: CMAC_SecurityMode_Config_CNF
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 2
- Message Structure:
CMAC_SecurityMode_Config_CNF
. (IntegerType)cellId = 0
- Constraint:
ca_CMAC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 00

- No.: 852
- Timestamp: 21:06:25:191_0
- RFN: 1124
- Chip: 17408
- Event: Send
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_REQ
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 3
- Message Structure:
CRLC_SecurityMode_Config_REQ
. (IntegerType)cellId = -1
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity = 0
. . (BitStringType)startValue[20] = "00000000000000000010"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = -
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CRLC_SecurityModeCfgReq
- BinaryMessage:
30 0e 02 01 ff 30 09 0a 01 00 03 04 04 00 00 20

- No.: 853
- Timestamp: 21:06:25:192_0
- RFN: 1124
- Chip: 23296
- Event: Receive
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_CNF
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 4
- Message Structure:
CRLC_SecurityMode_Config_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 860
- Timestamp: 21:06:25:202_0
- RFN: 1125
- Chip: 23808
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_GMM_IdleUpdated:lt_IdleUpdated_NMO_II LINE 3
- Message Structure:
RRC_DataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain = 0
. (START_Value)start[20] = '00000000000000000010'B
. LOCATIONUPDATINGREQUEST
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)mMProtocolDiscriminator[4] = '0101'B
. . (MsgType)msgType[8] = '00001000'B
. . CiphKeySeqNum
. . . (B1)spare1[1] = '0'B
. . . (KeySeq)keySeq[3] = '000'B
. . LocUpdType
. . . (B1)fOR[1] = '0'B
. . . (B1)spare1[1] = '0'B
. . . (B2)lUT[2] = '10'B
. . LocAreaId_v
. . . (OctetStringType)plmn[3] = '00F110'O
. . . (OctetStringType)lac[2] = '0001'O
. . MS_Clsmk1
. . . (B1)spare1[1] = '0'B
. . . (B2)revLvl[2] = '10'B
. . . (B1)eSIND[1] = '0'B
. . . (B1)a5_1[1] = '1'B
. . . (B3)rFPwrCap[3] = '111'B
. . MS_Identity_lv
. . . (Length)iel[1] = '05'O
. . . (B4)iDigit1[4] = '1111'B
. . . (B1)oddEvenInd[1] = '0'B
. . . (B3)typeOfId[3] = '100'B
. . . (OctetStringType)otherDigits[4] = '12345678'O
. . MS_Clsmk2
. . . (IEI8)iei[8] = '00110011'B
. . . (Length)iel[1] = '03'O
. . . (B1)spare1_1[1] = '0'B
. . . (B2)revLvl[2] = '10'B
. . . (B1)eSIND[1] = '0'B
. . . (B1)a5_1[1] = '1'B
. . . (B3)rFPwrCap[3] = '111'B
. . . (B1)spare1_2[1] = '0'B
. . . (B1)pSCap[1] = '0'B
. . . (B2)sSSI[2] = '01'B
. . . (B1)sMCap[1] = '1'B
. . . (B1)vBS[1] = '0'B
. . . (B1)vGCS[1] = '0'B
. . . (B1)fC[1] = '0'B
. . . (B1)cM3[1] = '1'B
. . . (B1)spare1_3[1] = '0'B
. . . (B1)lCSVA[1] = '0'B
. . . (B1)uCS2[1] = '0'B
. . . (B1)soLSA[1] = '0'B
. . . (B1)cMSP[1] = '0'B
. . . (B1)a5_3[1] = '0'B
. . . (B1)a5_2[1] = '0'B
- Constraint:
car_InitDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 00 03 04 04 00 00 20 05 08 02 00 f1 10 00 01 4f 05 f4 12 34 56 78 33 03 4f 18 80

- No.: 897
- Timestamp: 21:06:25:226_0
- RFN: 1127
- Chip: 36096
- Event: Send
- PCO: Dc
- Message: RRC_DataReq
- Source: ts_MM_Authentication LINE 2
- Message Structure:
RRC_DataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[-1] = -
. (SapId)sapId[1] = -
. (SS_CN_DomainIdentity)cN_Domain = 0
. AUTHENTICATIONREQUEST
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)mMProtocolDiscriminator[4] = '0101'B
. . (MsgType)msgType[8] = '00010010'B
. . (B4)spare4[4] = '0000'B
. . CiphKeySeqNum
. . . (B1)spare1[1] = '0'B
. . . (KeySeq)keySeq[3] = '000'B
. . (MM_RAND)rAND[128] = '01010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101'B
. . AUTN
. . . (IEI8)iei[8] = '00100000'B
. . . (Length)iel[1] = '10'O
. . . (BitStringType)aUTN[128] = '01010110010100010101000001010011010100100101110100000000000000000101010101010100010101110101011001010001010100000101001101010010'B
- Constraint:
ca_DataReq
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 00 05 12 00 55 55 55 55 55 55 55 55 55 55 55 55 55 55 55 55 20 10 56 51 50 53 52 5d 00 00 55 54 57 56 51 50 53 52

- No.: 901
- Timestamp: 21:06:25:860_0
- RFN: 1191
- Chip: 15872
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_MM_Authentication LINE 7
- Message Structure:
RRC_DataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain = 0
. (START_Value)start[0] = -
. AUTHENTICATIONRESPONSE
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)mMProtocolDiscriminator[4] = '0101'B
. . (MsgType)msgType[8] = '01010100'B
. . (AuthRsp)authRsp[32] = '01010101010101000101011101010110'B
. . AuthRspExt
- Constraint:
car_UplinkDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 00 05 54 55 54 57 56

- No.: 939
- Timestamp: 21:06:25:874_0
- RFN: 1192
- Chip: 32000
- Event: Send
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_REQ
- Source: ts_SS_DownloadSecurityKey:lt_DownloadKeyCRLC LINE 1
- Message Structure:
CRLC_SecurityMode_Config_REQ
. (IntegerType)cellId = -1
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity = 0
. . (BitStringType)startValue[20] = "00000000000000000000"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = '01010111010101100101000101010000010100110101001001011101010111000101111101011110010110010101100001011011010110100101010101010100'B
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CRLC_SecurityModeCfgReq
- BinaryMessage:
30 21 02 01 ff 30 1c 0a 01 00 03 04 04 00 00 00 03 11 00 57 56 51 50 53 52 5d 5c 5f 5e 59 58 5b 5a 55 54

- No.: 940
- Timestamp: 21:06:25:876_0
- RFN: 1193
- Chip: 1024
- Event: Receive
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_CNF
- Source: ts_SS_DownloadSecurityKey:lt_DownloadKeyCRLC LINE 2
- Message Structure:
CRLC_SecurityMode_Config_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 947
- Timestamp: 21:06:25:880_0
- RFN: 1193
- Chip: 13824
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 1
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
. (IntegerType)count_I_LSB_UL = -
. (IntegerType)count_I_LSB_DL = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 00 02 01 00 02 01 00

- No.: 948
- Timestamp: 21:06:25:882_0
- RFN: 1193
- Chip: 21248
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 2
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 00 02 01 00

- No.: 949
- Timestamp: 21:06:25:883_0
- RFN: 1193
- Chip: 28416
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 3
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. (IntegerType)count_I_LSB_UL = -
. (IntegerType)count_I_LSB_DL = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 01 02 01 00

- No.: 950
- Timestamp: 21:06:25:885_0
- RFN: 1193
- Chip: 35584
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 4
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 951
- Timestamp: 21:06:25:887_0
- RFN: 1194
- Chip: 4096
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 5
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. (IntegerType)count_I_LSB_UL = -
. (IntegerType)count_I_LSB_DL = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 02 02 01 00

- No.: 952
- Timestamp: 21:06:25:889_0
- RFN: 1194
- Chip: 12800
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 6
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 953
- Timestamp: 21:06:25:891_0
- RFN: 1194
- Chip: 20224
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 7
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
. (IntegerType)count_I_LSB_UL = -
. (IntegerType)count_I_LSB_DL = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 03 02 01 00

- No.: 954
- Timestamp: 21:06:25:893_0
- RFN: 1194
- Chip: 27648
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 8
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 955
- Timestamp: 21:06:25:895_0
- RFN: 1194
- Chip: 34560
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 9
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
. (IntegerType)count_I_LSB_UL = -
. (IntegerType)count_I_LSB_DL = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 04 02 01 00

- No.: 956
- Timestamp: 21:06:25:897_0
- RFN: 1195
- Chip: 3328
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 10
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 960
- Timestamp: 21:06:25:900_0
- RFN: 1195
- Chip: 15360
- Event: Send
- PCO: CRLC
- Message: CRLC_Integrity_Activate_REQ
- Source: ts_CRLC_DL_Integrity LINE 1
- Message Structure:
CRLC_Integrity_Activate_REQ
. (IntegerType)cellId = -1
. (CN_DomainIdentity)cn_DomainIdentity = 0
. IntegrityActivationInfo
. . IntegrityProtectionModeInfo
. . . IntegrityProtectionModeCommand
. . . . startIntegrityProtection
. . . . . (BitStringType)integrityProtInitNumber[32] = "00000000000000000000000000000001"
. . . (IntegrityProtectionAlgorithm)integrityProtectionAlgorithm = 0
- Constraint:
ca_CRLC_DL_IntegrityActivateReq
- BinaryMessage:
30 15 02 01 ff 0a 01 00 30 0d 30 30 07 03 05 00 00 00 00 01 0a 01 00

- No.: 961
- Timestamp: 21:06:25:902_0
- RFN: 1195
- Chip: 21760
- Event: Receive
- PCO: CRLC
- Message: CRLC_Integrity_Activate_CNF
- Source: ts_CRLC_DL_Integrity LINE 2
- Message Structure:
CRLC_Integrity_Activate_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_IntegrityActivateCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 968
- Timestamp: 21:06:25:905_0
- RFN: 1195
- Chip: 36608
- Event: Send
- PCO: CRLC
- Message: CRLC_Integrity_Activate_REQ
- Source: ts_RB2_UL_IntegrityActivate LINE 1
- Message Structure:
CRLC_Integrity_Activate_REQ
. (IntegerType)cellId = -1
. (CN_DomainIdentity)cn_DomainIdentity = 0
. IntegrityActivationInfo
. . IntegrityProtActivationInfoList
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity = 2
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
- Constraint:
ca_CRLC_UL_IntegrityActivateReq
- BinaryMessage:
30 10 02 01 ff 0a 01 00 30 08 30 06 02 01 02 02 01 00

- No.: 969
- Timestamp: 21:06:25:907_0
- RFN: 1196
- Chip: 4352
- Event: Receive
- PCO: CRLC
- Message: CRLC_Integrity_Activate_CNF
- Source: ts_RB2_UL_IntegrityActivate LINE 2
- Message Structure:
CRLC_Integrity_Activate_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_IntegrityActivateCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 975
- Timestamp: 21:06:25:913_0
- RFN: 1196
- Chip: 28672
- Event: Send
- PCO: AM
- Message: RLC_AM_DATA_REQ
- Source: ts_RRC_Security:lt_SendSecurityModeCommand LINE 7
- Message Structure:
RLC_AM_DATA_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. AmConfirmationRequest
. aM_message
. . DL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00000000000000000000000000000000"
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . DL_DCCH_MessageType
. . . . SecurityModeCommand
. . . . . r3
. . . . . . SecurityModeCommand_r3_IEs
. . . . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . . . SecurityCapability
. . . . . . . . (BitStringType)cipheringAlgorithmCap[16] = '0000000000000011'B
. . . . . . . . (BitStringType)integrityProtectionAlgorithmCap[16] = '0000000000000010'B
. . . . . . . CipheringModeInfo
. . . . . . . IntegrityProtectionModeInfo
. . . . . . . . IntegrityProtectionModeCommand
. . . . . . . . . startIntegrityProtection
. . . . . . . . . . (BitStringType)integrityProtInitNumber[32] = "00000000000000000000000000000001"
. . . . . . . . (IntegrityProtectionAlgorithm)integrityProtectionAlgorithm = 0
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity = 0
. . . . . . . InterRAT_UE_SecurityCapList
. . . . . . laterNonCriticalExtensions
- Constraint:
cas_RRC_SecModeCmd
- BinaryMessage:
30 17 02 01 ff 02 01 02 05 00 80 00 00 00 04 04 00 01 80 01 40 00 00 00 20

- No.: 981
- Timestamp: 21:06:26:039_0
- RFN: 1209
- Chip: 14336
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_IND
- Source: ts_RRC_Security:lt_StartSecurity_UE LINE 8
- Message Structure:
RLC_AM_DATA_IND
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. IntegrityResult
. . (IntegrityStatus)integrityUsed = 0
. aM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "10000001100000001110110111011101"
. . . . (IntegerType)rrc_MessageSequenceNumber = 1
. . . UL_DCCH_MessageType
. . . . SecurityModeComplete
. . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . IntegrityProtActivationInfo
. . . . . . RRC_MessageSequenceNumberList
. . . . . . . (IntegerType)_elem = 0
. . . . . . . (IntegerType)_elem = 0
. . . . . . . (IntegerType)_elem = 0
. . . . . . . (IntegerType)_elem = 0
. . . . . . . (IntegerType)_elem = 0
. . . . . laterNonCriticalExtensions
. . . . . . (BitStringType)securityModeComplete_r3_add_ext = 0
. . . . . . nonCriticalExtensions
- Constraint:
car_RRC_SecModeCmpl
- BinaryMessage:
30 12 02 01 ff 02 01 02 0a 01 00 c0 c0 76 ee 8d 21 00 00 00

- No.: 982
- Timestamp: 21:06:26:040_0
- RFN: 1209
- Chip: 18688
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_Security:lt_StartSecurity_UE LINE 8
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 984
- Timestamp: 21:06:26:045_0
- RFN: 1209
- Chip: 34304
- Event: Send
- PCO: CRLC
- Message: CRLC_Integrity_Activate_REQ
- Source: ts_CRLC_UL_Integrity LINE 1
- Message Structure:
CRLC_Integrity_Activate_REQ
. (IntegerType)cellId = -1
. (CN_DomainIdentity)cn_DomainIdentity = 0
. IntegrityActivationInfo
. . IntegrityProtActivationInfoList
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity = 0
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity = 1
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity = 3
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity = 4
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
- Constraint:
ca_CRLC_UL_IntegrityActivateReq
- BinaryMessage:
30 28 02 01 ff 0a 01 00 30 20 30 06 02 01 00 02 01 00 30 06 02 01 01 02 01 00 30 06 02 01 03 02 01 00 30 06 02 01 04 02 01 00

- No.: 985
- Timestamp: 21:06:26:046_0
- RFN: 1210
- Chip: 3328
- Event: Receive
- PCO: CRLC
- Message: CRLC_Integrity_Activate_CNF
- Source: ts_CRLC_UL_Integrity LINE 2
- Message Structure:
CRLC_Integrity_Activate_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_IntegrityActivateCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 992
- Timestamp: 21:06:26:052_0
- RFN: 1210
- Chip: 23040
- Event: Send
- PCO: Dc
- Message: RRC_DataReq
- Source: ts_GMM_IdleUpdated:lt_LocUpdAcc LINE 2
- Message Structure:
RRC_DataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[-1] = -
. (SapId)sapId[1] = -
. (SS_CN_DomainIdentity)cN_Domain = 0
. LOCATIONUPDATINGACCEPT
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)mMProtocolDiscriminator[4] = '0101'B
. . (MsgType)msgType[8] = '00000010'B
. . LocAreaId_v
. . . (OctetStringType)plmn[3] = '00F110'O
. . . (OctetStringType)lac[2] = '0001'O
. . MM_MS_Identity
. . . (IEI8)iei[8] = '00010111'B
. . . (Length)iel[1] = '05'O
. . . (B4)iDigit1[4] = '1111'B
. . . (B1)oddEvenInd[1] = '0'B
. . . (B3)typeOfId[3] = '100'B
. . . (OctetStringType)otherDigits[-1] = '12345678'O
. . (FollowOnProceed)followOnProceed[8] = '10100001'B
. . (CTSPerm)cTSPerm[8] = '10100010'B
. . PLMN_List
- Constraint:
ca_DataReq
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 00 05 02 00 f1 10 00 01 17 05 f4 12 34 56 78 a1 a2

- No.: 996
- Timestamp: 21:06:26:197_0
- RFN: 1225
- Chip: 4608
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_GMM_IdleUpdated:lt_LocUpdAcc LINE 3
- Message Structure:
RRC_DataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain = 0
. (START_Value)start[0] = -
. TMSIREALLOCATIONCOMPLETE
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)mMProtocolDiscriminator[4] = '0101'B
. . (MsgType)msgType[8] = '10011011'B
- Constraint:
car_UplinkDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 00 05 9b

- No.: 1010
- Timestamp: 21:06:26:202_0
- RFN: 1225
- Chip: 22016
- Event: Start Timer
- Source: ts_RRC_Delay LINE 1
- Message Structure:
no details available
- Constraint:
t_Dly (1000 Ms)
- BinaryMessage:

- No.: 1014
- Timestamp: 21:06:27:195_0
- RFN: 1324
- Chip: 35328
- Event: Timeout
- Source: ts_RRC_Delay LINE 2
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 1019
- Timestamp: 21:06:27:201_0
- RFN: 1325
- Chip: 18432
- Event: Send
- PCO: UM
- Message: RLC_UM_DATA_REQ
- Source: ts_RRC_ConnRel:lt_Send_RRC_ConnectionRelease LINE 3
- Message Structure:
RLC_UM_DATA_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. uM_message
. . DL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00000000000000000000000000000000"
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . DL_DCCH_MessageType
. . . . RRCConnectionRelease
. . . . . r3
. . . . . . RRCConnectionRelease_r3_IEs
. . . . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . . . (IntegerType)n_308 = 1
. . . . . . . (ReleaseCause)releaseCause = 0
. . . . . . . Rplmn_Information
. . . . . . laterNonCriticalExtensions
. (BooleanType)specialLI = FALSE
- Constraint:
cas_RRC_ConnRelDCCH
- BinaryMessage:
30 10 02 01 ff 02 01 01 80 00 00 00 03 c8 00 01 01 00

- No.: 1023
- Timestamp: 21:06:27:328_0
- RFN: 1338
- Chip: 9728
- Event: Receive
- PCO: UM
- Message: RLC_UM_DATA_IND
- Source: ts_RRC_ConnRel:lt_Send_RRC_ConnectionRelease LINE 4
- Message Structure:
RLC_UM_DATA_IND
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. IntegrityResult
. uM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "10101101101011101001000000111001"
. . . . (IntegerType)rrc_MessageSequenceNumber = 1
. . . UL_DCCH_MessageType
. . . . RRCConnectionReleaseComplete
. . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . FailureCauseWithProtErr
. . . . . laterNonCriticalExtensions
. . . . . . (BitStringType)rrcConnectionReleaseComplete_r3_add_ext = 0
. . . . . . nonCriticalExtensions
- Constraint:
car_RRC_ConnRelCmplUM
- BinaryMessage:
30 0c 02 01 ff 02 01 01 d6 d7 48 1c 8c 40

- No.: 1024
- Timestamp: 21:06:27:329_0
- RFN: 1338
- Chip: 13312
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ConnRel:lt_Send_RRC_ConnectionRelease LINE 4
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1027
- Timestamp: 21:06:27:330_2
- RFN: 1338
- Chip: 18688
- Event: Start Timer
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 1
- Message Structure:
no details available
- Constraint:
t_Dly (5000 Ms)
- BinaryMessage:

- No.: 1031
- Timestamp: 21:06:27:478_0
- RFN: 1353
- Chip: 8448
- Event: Receive
- PCO: UM
- Message: RLC_UM_DATA_IND
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 4
- Message Structure:
RLC_UM_DATA_IND
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. IntegrityResult
. uM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00011100010101000111110101101001"
. . . . (IntegerType)rrc_MessageSequenceNumber = 2
. . . UL_DCCH_MessageType
. . . . RRCConnectionReleaseComplete
. . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . FailureCauseWithProtErr
. . . . . laterNonCriticalExtensions
. . . . . . (BitStringType)rrcConnectionReleaseComplete_r3_add_ext = 0
. . . . . . nonCriticalExtensions
- Constraint:
car_RRC_ConnRelCmplUM
- BinaryMessage:
30 0c 02 01 ff 02 01 01 8e 2a 3e b4 94 40

- No.: 1032
- Timestamp: 21:06:27:479_0
- RFN: 1353
- Chip: 12288
- Event: Cancel Timer
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 4
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 1033
- Timestamp: 21:06:27:479_1
- RFN: 1353
- Chip: 13312
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 4
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1039
- Timestamp: 21:06:27:483_0
- RFN: 1353
- Chip: 27904
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 01 0a 01 00 05 00

- No.: 1043
- Timestamp: 21:06:27:489_0
- RFN: 1354
- Chip: 13312
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 1046
- Timestamp: 21:06:27:493_0
- RFN: 1354
- Chip: 25344
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 02 0a 01 00 05 00

- No.: 1050
- Timestamp: 21:06:27:500_0
- RFN: 1355
- Chip: 15104
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 1053
- Timestamp: 21:06:27:502_0
- RFN: 1355
- Chip: 25088
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 03 0a 01 00 05 00

- No.: 1057
- Timestamp: 21:06:27:514_0
- RFN: 1356
- Chip: 30976
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 1060
- Timestamp: 21:06:27:517_0
- RFN: 1357
- Chip: 4864
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 04 0a 01 00 05 00

- No.: 1064
- Timestamp: 21:06:27:529_0
- RFN: 1358
- Chip: 13312
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 1067
- Timestamp: 21:06:27:536_0
- RFN: 1359
- Chip: 2560
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 136
. . . . . UL_RLC_Mode
. . . . . . UL_UM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (NoExplicitDiscard)timerBasedNoExplicit = 9
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = 1
. . . . (IntegerType)dLlogicalChannelIdentity = 1
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_UM_Info
- BinaryMessage:
30 22 02 01 ff 02 01 01 0a 01 00 30 17 30 0d 05 00 30 09 02 02 00 88 30 03 0a 01 09 30 06 02 01 01 02 01 01

- No.: 1071
- Timestamp: 21:06:27:547_0
- RFN: 1360
- Chip: 5632
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 1072
- Timestamp: 21:06:27:556_0
- RFN: 1361
- Chip: 256
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 3
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . (TimerEPC)timerEPC = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . (TimerRST)timerRST = 9
. . . . . . . (MaxRST)max_RST = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = 2
. . . . (IntegerType)dLlogicalChannelIdentity = 2
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 02 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 27 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 02 02 01 02

- No.: 1076
- Timestamp: 21:06:27:577_0
- RFN: 1363
- Chip: 6400
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 4
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 1077
- Timestamp: 21:06:27:586_0
- RFN: 1364
- Chip: 0
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 5
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . (TimerEPC)timerEPC = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . (TimerRST)timerRST = 9
. . . . . . . (MaxRST)max_RST = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = 3
. . . . (IntegerType)dLlogicalChannelIdentity = 3
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 03 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 27 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 03 02 01 03

- No.: 1081
- Timestamp: 21:06:27:603_0
- RFN: 1365
- Chip: 29696
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 6
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 1082
- Timestamp: 21:06:27:612_0
- RFN: 1366
- Chip: 26112
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 7
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . (TimerEPC)timerEPC = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . (TimerRST)timerRST = 9
. . . . . . . (MaxRST)max_RST = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = 4
. . . . (IntegerType)dLlogicalChannelIdentity = 4
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 04 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 27 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 04 02 01 04

- No.: 1086
- Timestamp: 21:06:27:634_0
- RFN: 1368
- Chip: 34304
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 8
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 1109
- Timestamp: 21:06:27:642_1
- RFN: 1369
- Chip: 25344
- Event: Start Timer
- Source: ts_GMM_IdleUpdated:lt_HandleAttachRequest LINE 5
- Message Structure:
no details available
- Constraint:
t_WaitS (1 Sec)
- BinaryMessage:

- No.: 1113
- Timestamp: 21:06:28:632_0
- RFN: 1468
- Chip: 26112
- Event: Timeout
- Source: ts_GMM_IdleUpdated:lt_HandleAttachRequest LINE 6
- Message Structure:
no details available
- Constraint:
t_WaitS
- BinaryMessage:

- No.: 1115
- Timestamp: 21:06:28:634_0
- RFN: 1468
- Chip: 28672
- Event: Start Timer
- Source: ts_GMM_IdleUpdated:lt_HandleAttachRequest LINE 7
- Message Structure:
no details available
- Constraint:
t_WaitS (60 Sec)
- BinaryMessage:

- No.: 1117
- Timestamp: 21:06:28:636_0
- RFN: 1468
- Chip: 36608
- Event: Send
- PCO: Ut
- Message: AT_CmdReq
- Source: ts_AT_TriggerGMM_Attach LINE 1
- Message Structure:
AT_CmdReq
. (IA5StringType)cmd[-1] = "AT+CGATT=1"
. (HexStringType)sMS_BlockMode[-1] = -
- Constraint:
ca_AT_CmdReq
- BinaryMessage:
41 54 2b 43 47 41 54 54 3d 31 3c 43 52 3e

- No.: 1121
- Timestamp: 21:06:29:765_0
- RFN: 1581
- Chip: 35584
- Event: Receive
- PCO: Ut
- Message: AT_CmdCnf
- Source: ts_AT_TriggerGMM_Attach LINE 2
- Message Structure:
AT_CmdCnf
. (BooleanType)result = TRUE
. (IA5StringType)resultString[18] = "OK"
. (HexStringType)sMS_BlockMode[0] = -
- Constraint:
ca_AT_CmdCnf
- BinaryMessage:
80 3c 43 52 3e 3c 4c 46 3e 4f 4b 3c 43 52 3e 3c 4c 46 3e

- No.: 1138
- Timestamp: 21:06:29:772_0
- RFN: 1582
- Chip: 23296
- Event: Receive
- PCO: CPHY
- Message: CPHY_Out_of_Sync_IND
- Source: RRC_DefConnEst LINE 7
- Message Structure:
CPHY_Out_of_Sync_IND
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_OutOfSyncInd
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 1139
- Timestamp: 21:06:29:772_1
- RFN: 1582
- Chip: 25088
- Event: Cancel Timer
- Source: RRC_DefConnEst LINE 7
- Message Structure:
no details available
- Constraint:
t_T312
- BinaryMessage:

- No.: 1140
- Timestamp: 21:06:29:773_0
- RFN: 1582
- Chip: 27136
- Event: Default
- Source: RRC_DefConnEst LINE 0
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1141
- Timestamp: 21:06:29:773_1
- RFN: 1582
- Chip: 27904
- Event: Default
- Source: ts_RRC_ConnEst:lt_RcvConnReq LINE 2
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1146
- Timestamp: 21:06:31:368_0
- RFN: 1742
- Chip: 9984
- Event: Receive
- PCO: TM
- Message: RLC_TR_DATA_IND
- Source: ts_RRC_ConnEst:lt_RcvConnReq LINE 2
- Message Structure:
RLC_TR_DATA_IND
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
. tM_message
. . UL_CCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode = 0
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . UL_CCCH_MessageType
. . . . RRCConnectionRequest
. . . . . InitialUE_Identity
. . . . . . TMSI_and_LAI_GSM_MAP
. . . . . . . (BitStringType)tmsi[32] = "00010010001101000101011001111000"
. . . . . . . LAI
. . . . . . . . PLMN_Identity
. . . . . . . . . MCC
. . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . (IntegerType)_elem = 1
. . . . . . . . . MNC
. . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . (IntegerType)_elem = 1
. . . . . . . . (BitStringType)lac[16] = '0000000000000001'B
. . . . . (EstablishmentCause)establishmentCause = 12
. . . . . (ProtocolErrorIndicator)protocolErrorIndicator = 0
. . . . . MeasuredResultsOnRACH
. . . . . . currentCell
. . . . . . . modeSpecificInfo
. . . . . . . . fdd
. . . . . . . . . measurementQuantity
. . . . . . . . . . (IntegerType)cpich_Ec_N0 = 0
. . . . . v3d0NonCriticalExtensions
. . . . . . RRCConnectionRequest_v3d0ext_IEs
. . . . . . . (BitStringType)uESpecificBehaviourInformation1idle = 0
. . . . . . nonCriticalExtensions
- Constraint:
car_RRC_ConnReq
- BinaryMessage:
30 11 02 01 00 02 01 00 21 12 34 56 78 00 10 08 00 0b 00

- No.: 1150
- Timestamp: 21:06:31:429_0
- RFN: 1748
- Chip: 12544
- Event: Send
- PCO: UM
- Message: RLC_UM_DATA_REQ
- Source: ts_RRC_ConnEst:lt_Send_ConnSetUp LINE 22
- Message Structure:
RLC_UM_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
. uM_message
. . DL_CCCH_Message
. . . IntegrityCheckInfo
. . . DL_CCCH_MessageType
. . . . RRCConnectionSetup
. . . . . r3
. . . . . . RRCConnectionSetup_r3_IEs
. . . . . . . InitialUE_Identity
. . . . . . . . TMSI_and_LAI_GSM_MAP
. . . . . . . . . (BitStringType)tmsi[32] = "00010010001101000101011001111000"
. . . . . . . . . LAI
. . . . . . . . . . PLMN_Identity
. . . . . . . . . . . MCC
. . . . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . . . (IntegerType)_elem = 1
. . . . . . . . . . . MNC
. . . . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . . . (IntegerType)_elem = 1
. . . . . . . . . . (BitStringType)lac[16] = '0000000000000001'B
. . . . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . . . (IntegerType)activationTime = -
. . . . . . . U_RNTI
. . . . . . . . (BitStringType)srnc_Identity[12] = "000000000001"
. . . . . . . . (BitStringType)s_RNTI[20] = "00000000000000000001"
. . . . . . . (BitStringType)new_c_RNTI[16] = -
. . . . . . . (RRC_StateIndicator)rrc_StateIndicator = 0
. . . . . . . (IntegerType)utran_DRX_CycleLengthCoeff = 9
. . . . . . . CapabilityUpdateRequirement
. . . . . . . . (BooleanType)ue_RadioCapabilityFDDUpdateRequirement = TRUE
. . . . . . . . (BooleanType)ue_RadioCapabilityTDDUpdateRequirement = FALSE
. . . . . . . . SystemSpecificCapUpdateReqList
. . . . . . . . . (SystemSpecificCapUpdateReq)_elem = 0
. . . . . . . SRB_InformationSetupList2
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_UM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 1
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 1
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . . . . . . . (TimerRST)timerRST = 9
. . . . . . . . . . . . . (MaxRST)max_RST = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 2
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 2
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . . . . . . . (TimerRST)timerRST = 9
. . . . . . . . . . . . . (MaxRST)max_RST = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 3
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 3
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . . . . . . . (TimerRST)timerRST = 9
. . . . . . . . . . . . . (MaxRST)max_RST = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 4
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 4
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . UL_CommonTransChInfo
. . . . . . . . TFC_Subset
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . TFCS
. . . . . . . . . . . ExplicitTFCS_Configuration
. . . . . . . . . . . . TFCS_ReconfAdd
. . . . . . . . . . . . . ctfcSize
. . . . . . . . . . . . . . ctfc2Bit
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . . . . . . . (IntegerType)ctfc2 = 0
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . . . . . . . (IntegerType)ctfc2 = 1
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 11
. . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . UL_AddReconfTransChInfoList
. . . . . . . . UL_AddReconfTransChInformation
. . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType = 0
. . . . . . . . . (IntegerType)transportChannelIdentity = 5
. . . . . . . . . TransportFormatSet
. . . . . . . . . . DedicatedTransChTFS
. . . . . . . . . . . tti
. . . . . . . . . . . . DedicatedDynamicTF_InfoList
. . . . . . . . . . . . . DedicatedDynamicTF_Info
. . . . . . . . . . . . . . rlc_Size
. . . . . . . . . . . . . . . BitModeRLC_SizeInfo
. . . . . . . . . . . . . . . . sizeType2
. . . . . . . . . . . . . . . . . (IntegerType)part1 = 2
. . . . . . . . . . . . . . . . . (IntegerType)part2 = -
. . . . . . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . LogicalChannelList
. . . . . . . . . . . SemistaticTF_Information
. . . . . . . . . . . . ChannelCodingType
. . . . . . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . . . . . (IntegerType)rateMatchingAttribute = 192
. . . . . . . . . . . . (CRC_Size)crc_Size = 3
. . . . . . . DL_CommonTransChInfo
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . dl_Parameters
. . . . . . . DL_AddReconfTransChInfoList
. . . . . . . . DL_AddReconfTransChInformation
. . . . . . . . . (DL_TrCH_Type)dl_TransportChannelType = 0
. . . . . . . . . (IntegerType)dl_transportChannelIdentity = 10
. . . . . . . . . tfs_SignallingMode
. . . . . . . . . . UL_TransportChannelIdentity
. . . . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType = 0
. . . . . . . . . . . (IntegerType)ul_TransportChannelIdentity = 5
. . . . . . . . . QualityTarget
. . . . . . . . . . (IntegerType)bler_QualityValue = -20
. . . . . . . . . TM_SignallingInfo
. . . . . . . FrequencyInfo
. . . . . . . (IntegerType)maxAllowedUL_TX_Power = -
. . . . . . . UL_ChannelRequirement
. . . . . . . . UL_DPCH_Info
. . . . . . . . . UL_DPCH_PowerControlInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (IntegerType)dpcch_PowerOffset = -40
. . . . . . . . . . . (IntegerType)pc_Preamble = 1
. . . . . . . . . . . (IntegerType)sRB_delay = 7
. . . . . . . . . . . PowerControlAlgorithm
. . . . . . . . . . . . (IntegerType)algorithm1 = 1
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (ScramblingCodeType)scramblingCodeType = 1
. . . . . . . . . . . (IntegerType)scramblingCode = 0
. . . . . . . . . . . (IntegerType)numberOfDPDCH = -
. . . . . . . . . . . (SpreadingFactor)spreadingFactor = 4
. . . . . . . . . . . (BooleanType)tfci_Existence = TRUE
. . . . . . . . . . . (IntegerType)numberOfFBI_Bits = -
. . . . . . . . . . . (PuncturingLimit)puncturingLimit = 15
. . . . . . . DL_CommonInformation
. . . . . . . . DL_DPCH_InfoCommon
. . . . . . . . . cfnHandling
. . . . . . . . . . initialise
. . . . . . . . . . . (IntegerType)cfntargetsfnframeoffset = -
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . DL_DPCH_PowerControlInfo
. . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . (DPC_Mode)dpc_Mode = 0
. . . . . . . . . . . (IntegerType)powerOffsetPilot_pdpdch = 0
. . . . . . . . . . . Dl_rate_matching_restriction
. . . . . . . . . . . SF512_AndPilot
. . . . . . . . . . . . (PilotBits128)sfd128 = 0
. . . . . . . . . . . (PositionFixedOrFlexible)positionFixedOrFlexible = 0
. . . . . . . . . . . (BooleanType)tfci_Existence = FALSE
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . (IntegerType)defaultDPCH_OffsetValue = 0
. . . . . . . . . . DPCH_CompressedModeInfo
. . . . . . . . . . (TX_DiversityMode)tx_DiversityMode = 0
. . . . . . . . . . SSDT_Information
. . . . . . . DL_InformationPerRL_List
. . . . . . . . DL_InformationPerRL
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . PrimaryCPICH_Info
. . . . . . . . . . . . (IntegerType)primaryScramblingCode = 100
. . . . . . . . . . . PDSCH_SHO_DCH_Info
. . . . . . . . . . . PDSCH_CodeMapping
. . . . . . . . . DL_DPCH_InfoPerRL
. . . . . . . . . . fdd
. . . . . . . . . . . (PCPICH_UsageForChannelEst)pCPICH_UsageForChannelEst = 0
. . . . . . . . . . . (IntegerType)dpch_FrameOffset = 0
. . . . . . . . . . . SecondaryCPICH_Info
. . . . . . . . . . . DL_ChannelisationCodeList
. . . . . . . . . . . . DL_ChannelisationCode
. . . . . . . . . . . . . (IntegerType)secondaryScramblingCode = 1
. . . . . . . . . . . . . SF512_AndCodeNumber
. . . . . . . . . . . . . . (IntegerType)sf128 = 0
. . . . . . . . . . . . . (ScramblingCodeChange)scramblingCodeChange = 1
. . . . . . . . . . . (IntegerType)tpc_CombinationIndex = 0
. . . . . . . . . . . (SSDT_CellIdentity)ssdt_CellIdentity = -
. . . . . . . . . . . (ClosedLoopTimingAdjMode)closedLoopTimingAdjMode = -
. . . . . . . . . SCCPCH_InfoForFACH
. . . . . . laterNonCriticalExtensions
. (BooleanType)specialLI = TRUE
- Constraint:
cas_RRC_ConnSetup
- BinaryMessage:
30 78 02 01 00 02 01 00 30 e7 22 46 8a cf 00 02 01 00 01 00 04 00 00 4d 82 69 3a 10 10 89 0d 42 00 02 81 9e 8e 46 c9 ce 7c 9c 4e 74 20 a5 12 3a 8c 00 15 13 3d 1c 8d 93 9c f9 38 9c e8 42 52 24 b5 28 00 4a 46 7a 39 1b 27 39 f2 71 39 d0 86 b4 49 ea 70 00 d4 c8 00 06 25 2b f0 02 00 08 82 23 bf 66 08 98 95 a5 47 a2 00 00 01 3f 90 0a 14 00 02 06 40 00 0c 28 08 01 01 ff

- No.: 1171
- Timestamp: 21:06:31:473_0
- RFN: 1752
- Chip: 25088
- Event: Start Timer
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 3
- Message Structure:
no details available
- Constraint:
t_WaitMS (13500 Ms)
- BinaryMessage:

- No.: 1176
- Timestamp: 21:06:31:693_0
- RFN: 1774
- Chip: 29440
- Event: Receive
- PCO: CPHY
- Message: CPHY_Sync_IND
- Source: RRC_Def1 LINE 13
- Message Structure:
CPHY_Sync_IND
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_SyncInd
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 1177
- Timestamp: 21:06:31:694_0
- RFN: 1774
- Chip: 32768
- Event: Cancel Timer
- Source: RRC_Def1 LINE 13
- Message Structure:
no details available
- Constraint:
t_T312
- BinaryMessage:

- No.: 1178
- Timestamp: 21:06:31:695_0
- RFN: 1774
- Chip: 34560
- Event: Default
- Source: RRC_Def1 LINE 0
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1179
- Timestamp: 21:06:31:695_1
- RFN: 1774
- Chip: 35328
- Event: Default
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1184
- Timestamp: 21:06:31:809_0
- RFN: 1786
- Chip: 12288
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_IND
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
RLC_AM_DATA_IND
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. IntegrityResult
. . (IntegrityStatus)integrityUsed = 0
. aM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode = 0
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . UL_DCCH_MessageType
. . . . RRCConnectionSetupComplete
. . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . STARTList
. . . . . . STARTSingle
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity = 1
. . . . . . . (BitStringType)start_Value[20] = "00000000000000000100"
. . . . . . STARTSingle
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity = 0
. . . . . . . (BitStringType)start_Value[20] = "00000000000000000010"
. . . . . UE_RadioAccessCapability
. . . . . . (AccessStratumReleaseIndicator)accessStratumReleaseIndicator = 0
. . . . . . PDCP_Capability
. . . . . . . (BooleanType)losslessSRNS_RelocationSupport = FALSE
. . . . . . . supportForRfc2507
. . . . . . RLC_Capability
. . . . . . . (TotalRLC_AM_BufferSize)totalRLC_AM_BufferSize = 2
. . . . . . . (MaximumRLC_WindowSize)maximumRLC_WindowSize = 0
. . . . . . . (MaximumAM_EntityNumberRLC_Cap)maximumAM_EntityNumber = 3
. . . . . . TransportChannelCapability
. . . . . . . DL_TransChCapability
. . . . . . . . (MaxNoBits)maxNoBitsReceived = 4
. . . . . . . . (MaxNoBits)maxConvCodeBitsReceived = 1
. . . . . . . . TurboSupport
. . . . . . . . . (MaxNoBits)supported = 4
. . . . . . . . (MaxSimultaneousTransChsDL)maxSimultaneousTransChs = 1
. . . . . . . . (IntegerType)maxSimultaneousCCTrCH_Count = 1
. . . . . . . . (MaxTransportBlocksDL)maxReceivedTransportBlocks = 2
. . . . . . . . (MaxNumberOfTFC_DL)maxNumberOfTFC = 4
. . . . . . . . (MaxNumberOfTF)maxNumberOfTF = 1
. . . . . . . UL_TransChCapability
. . . . . . . . (MaxNoBits)maxNoBitsTransmitted = 3
. . . . . . . . (MaxNoBits)maxConvCodeBitsTransmitted = 1
. . . . . . . . TurboSupport
. . . . . . . . . (MaxNoBits)supported = 3
. . . . . . . . (MaxSimultaneousTransChsUL)maxSimultaneousTransChs = 2
. . . . . . . . modeSpecificInfo
. . . . . . . . (MaxTransportBlocksUL)maxTransmittedBlocks = 2
. . . . . . . . (MaxNumberOfTFC_UL)maxNumberOfTFC = 3
. . . . . . . . (MaxNumberOfTF)maxNumberOfTF = 0
. . . . . . RF_Capability
. . . . . . . fddRF_Capability
. . . . . . . . (IntegerType)ue_PowerClass = 4
. . . . . . . . (TxRxFrequencySeparation)txRxFrequencySeparation = 0
. . . . . . . tddRF_Capability
. . . . . . . . (IntegerType)ue_PowerClass = 0
. . . . . . . . (RadioFrequencyBandTDDList)radioFrequencyTDDBandList = 0
. . . . . . . . (ChipRateCapability)chipRateCapability = 0
. . . . . . PhysicalChannelCapability
. . . . . . . fddPhysChCapability
. . . . . . . . DL_PhysChCapabilityFDD
. . . . . . . . . (IntegerType)maxNoDPCH_PDSCH_Codes = 3
. . . . . . . . . (MaxNoPhysChBitsReceived)maxNoPhysChBitsReceived = 6
. . . . . . . . . (BooleanType)supportForSF_512 = FALSE
. . . . . . . . . (BooleanType)supportOfPDSCH = FALSE
. . . . . . . . . SimultaneousSCCPCH_DPCH_Reception
. . . . . . . . UL_PhysChCapabilityFDD
. . . . . . . . . (MaxNoDPDCH_BitsTransmitted)maxNoDPDCH_BitsTransmitted = 2
. . . . . . . . . (BooleanType)supportOfPCPCH = FALSE
. . . . . . . tddPhysChCapability
. . . . . . . . DL_PhysChCapabilityTDD
. . . . . . . . . (IntegerType)maxTS_PerFrame = 0
. . . . . . . . . (IntegerType)maxPhysChPerFrame = 0
. . . . . . . . . (MinimumSF_DL)minimumSF = 0
. . . . . . . . . (BooleanType)supportOfPDSCH = FALSE
. . . . . . . . . (IntegerType)maxPhysChPerTS = 0
. . . . . . . . UL_PhysChCapabilityTDD
. . . . . . . . . (IntegerType)maxTS_PerFrame = 0
. . . . . . . . . (MaxPhysChPerTimeslot)maxPhysChPerTimeslot = 0
. . . . . . . . . (MinimumSF_UL)minimumSF = 0
. . . . . . . . . (BooleanType)supportOfPUSCH = FALSE
. . . . . . UE_MultiModeRAT_Capability
. . . . . . . MultiRAT_Capability
. . . . . . . . (BooleanType)supportOfGSM = TRUE
. . . . . . . . (BooleanType)supportOfMulticarrier = FALSE
. . . . . . . (MultiModeCapability)multiModeCapability = 1
. . . . . . SecurityCapability
. . . . . . . (BitStringType)cipheringAlgorithmCap[16] = '0000000000000011'B
. . . . . . . (BitStringType)integrityProtectionAlgorithmCap[16] = '0000000000000010'B
. . . . . . UE_Positioning_Capability
. . . . . . . (BooleanType)standaloneLocMethodsSupported = FALSE
. . . . . . . (BooleanType)ue_BasedOTDOA_Supported = FALSE
. . . . . . . (NetworkAssistedGPS_Supported)networkAssistedGPS_Supported = 3
. . . . . . . (BooleanType)supportForUE_GPS_TimingOfCellFrames = FALSE
. . . . . . . (BooleanType)supportForIPDL = FALSE
. . . . . . MeasurementCapability
. . . . . . . CompressedModeMeasCapability
. . . . . . . . (BooleanType)fdd_Measurements = TRUE
. . . . . . . . (BooleanType)tdd_Measurements = FALSE
. . . . . . . . GSM_Measurements
. . . . . . . . . (BooleanType)gsm900 = TRUE
. . . . . . . . . (BooleanType)dcs1800 = TRUE
. . . . . . . . . (BooleanType)gsm1900 = FALSE
. . . . . . . . (BooleanType)multiCarrierMeasurements = FALSE
. . . . . . . CompressedModeMeasCapability
. . . . . . . . (BooleanType)fdd_Measurements = TRUE
. . . . . . . . (BooleanType)tdd_Measurements = FALSE
. . . . . . . . GSM_Measurements
. . . . . . . . . (BooleanType)gsm900 = TRUE
. . . . . . . . . (BooleanType)dcs1800 = TRUE
. . . . . . . . . (BooleanType)gsm1900 = FALSE
. . . . . . . . (BooleanType)multiCarrierMeasurements = FALSE
. . . . . v370NonCriticalExtensions
. . . . . . RRCConnectionSetupComplete_v370ext
. . . . . . . UE_RadioAccessCapability_v370ext
. . . . . . v380NonCriticalExtensions
. . . . . . . RRCConnectionSetupComplete_v380ext_IEs
. . . . . . . . UE_RadioAccessCapability_v380ext
. . . . . . . . . UE_PositioningCapabilityExt_v380
. . . . . . . . . . (BooleanType)rx_tx_TimeDifferenceType2Capable = FALSE
. . . . . . . . DL_PhysChCapabilityFDD_v380ext
. . . . . . . . . (SupportOfDedicatedPilotsForChEstimation)supportOfDedicatedPilotsForChEstimation = 0
. . . . . . . v3a0NonCriticalExtensions
. . . . . . . . RRCConnectionSetupComplete_v3a0ext_IEs
. . . . . . . . . UE_RadioAccessCapability_v3a0ext
. . . . . . . . . . UE_PositioningCapabilityExt_v3a0
. . . . . . . . . . . (UE_PositioningCapabilityExt_v3a0_list_0)validity_CellPCH_UraPCH = 0
. . . . . . . . laterNonCriticalExtensions
. . . . . . . . . (BitStringType)rrcConnectionSetupComplete_r3_add_ext = 0
. . . . . . . . . nonCriticalExtensions
- Constraint:
car_RRC_ConnSetupCmpl
- BinaryMessage:
30 27 02 01 ff 02 01 02 0a 05 01 00 00 00 00 4a 0c 00 01 00 00 05 11 a0 d1 04 84 c6 68 46 2c 93 02 48 00 18 00 11 8f 8f 80

- No.: 1185
- Timestamp: 21:06:31:817_0
- RFN: 1787
- Chip: 3584
- Event: Cancel Timer
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
t_WaitMS
- BinaryMessage:

- No.: 1186
- Timestamp: 21:06:31:817_1
- RFN: 1787
- Chip: 4608
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1200
- Timestamp: 21:06:31:826_0
- RFN: 1788
- Chip: 512
- Event: Send
- PCO: CMAC
- Message: CMAC_SecurityMode_Config_REQ
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 1
- Message Structure:
CMAC_SecurityMode_Config_REQ
. (IntegerType)cellId = 0
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity = 1
. . (BitStringType)startValue[20] = "00000000000000000100"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = -
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CMAC_SecurityModeCfgReq
- BinaryMessage:
30 0e 02 01 00 30 09 0a 01 01 03 04 04 00 00 40

- No.: 1201
- Timestamp: 21:06:31:828_0
- RFN: 1788
- Chip: 8704
- Event: Receive
- PCO: CMAC
- Message: CMAC_SecurityMode_Config_CNF
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 2
- Message Structure:
CMAC_SecurityMode_Config_CNF
. (IntegerType)cellId = 0
- Constraint:
ca_CMAC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 00

- No.: 1202
- Timestamp: 21:06:31:830_0
- RFN: 1788
- Chip: 16384
- Event: Send
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_REQ
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 3
- Message Structure:
CRLC_SecurityMode_Config_REQ
. (IntegerType)cellId = -1
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity = 1
. . (BitStringType)startValue[20] = "00000000000000000100"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = -
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CRLC_SecurityModeCfgReq
- BinaryMessage:
30 0e 02 01 ff 30 09 0a 01 01 03 04 04 00 00 40

- No.: 1203
- Timestamp: 21:06:31:832_0
- RFN: 1788
- Chip: 22528
- Event: Receive
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_CNF
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 4
- Message Structure:
CRLC_SecurityMode_Config_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1217
- Timestamp: 21:06:31:837_0
- RFN: 1789
- Chip: 3840
- Event: Send
- PCO: CMAC
- Message: CMAC_SecurityMode_Config_REQ
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 1
- Message Structure:
CMAC_SecurityMode_Config_REQ
. (IntegerType)cellId = 0
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity = 0
. . (BitStringType)startValue[20] = "00000000000000000010"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = -
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CMAC_SecurityModeCfgReq
- BinaryMessage:
30 0e 02 01 00 30 09 0a 01 00 03 04 04 00 00 20

- No.: 1218
- Timestamp: 21:06:31:839_0
- RFN: 1789
- Chip: 10240
- Event: Receive
- PCO: CMAC
- Message: CMAC_SecurityMode_Config_CNF
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 2
- Message Structure:
CMAC_SecurityMode_Config_CNF
. (IntegerType)cellId = 0
- Constraint:
ca_CMAC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 00

- No.: 1219
- Timestamp: 21:06:31:841_0
- RFN: 1789
- Chip: 17408
- Event: Send
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_REQ
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 3
- Message Structure:
CRLC_SecurityMode_Config_REQ
. (IntegerType)cellId = -1
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity = 0
. . (BitStringType)startValue[20] = "00000000000000000010"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = -
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CRLC_SecurityModeCfgReq
- BinaryMessage:
30 0e 02 01 ff 30 09 0a 01 00 03 04 04 00 00 20

- No.: 1220
- Timestamp: 21:06:31:842_0
- RFN: 1789
- Chip: 23552
- Event: Receive
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_CNF
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 4
- Message Structure:
CRLC_SecurityMode_Config_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1227
- Timestamp: 21:06:31:851_0
- RFN: 1790
- Chip: 20224
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_GMM_IdleUpdated:lt_HandleAttachRequest LINE 10
- Message Structure:
RRC_DataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. (START_Value)start[20] = '00000000000000000100'B
. ATTACHREQUEST
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)gMMProtocolDiscriminator[4] = '1000'B
. . (MsgType)msgType[8] = '00000001'B
. . MS_NetworkCap_lv
. . . (Length)iel[1] = '02'O
. . . (OctetStringType)value[2] = 'E540'O
. . CiphKeySeqNum
. . . (B1)spare1[1] = '0'B
. . . (KeySeq)keySeq[3] = '000'B
. . AttachType
. . . (B1)pre_for[1] = '0'B
. . . (B3)type[3] = '001'B
. . DRXparamter
. . . (B8)splitPGcycleCode[8] = '00000111'B
. . . (B4)cnDRXcoef[4] = '0000'B
. . . (B1)splitOnCCCH[1] = '0'B
. . . (B3)nonDRXtimer[3] = '010'B
. . MS_Identity_lv
. . . (Length)iel[1] = '05'O
. . . (B4)iDigit1[4] = '1111'B
. . . (B1)oddEvenInd[1] = '0'B
. . . (B3)typeOfId[3] = '100'B
. . . (OctetStringType)otherDigits[4] = '12345678'O
. . RAI_v
. . . (OctetStringType)plmn[3] = '00F110'O
. . . (OctetStringType)lac[2] = '0001'O
. . . (OctetStringType)rac[1] = '05'O
. . MSRadioAccessCap_lv
. . . (Length)iel[1] = '0A'O
. . . (OctetStringType)value[10] = '14F382334C03263CA060'O
. . PTMSI_Signature
. . . (IEI8)iei[8] = '00010111'B
. . . (OctetStringType)value[3] = -
. . GPRS_Timer
. . . (IEI8)iei[8] = '00010110'B
. . . (B3)unit[0] = -
. . . (B5)value[0] = -
. . TMSI_Status
. . . (IEI4)iei[0] = -
. . . (B3)spare3[0] = -
. . . (B1)flag[0] = -
- Constraint:
car_PS_InitDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 03 04 04 00 00 40 08 01 02 e5 40 01 07 02 05 f4 12 34 56 78 00 f1 10 00 01 05 0a 14 f3 82 33 4c 03 26 3c a0 60 17 16

- No.: 1228
- Timestamp: 21:06:31:856_0
- RFN: 1791
- Chip: 1280
- Event: Cancel Timer
- Source: ts_GMM_IdleUpdated:lt_HandleAttachRequest LINE 10
- Message Structure:
no details available
- Constraint:
t_WaitS
- BinaryMessage:

- No.: 1265
- Timestamp: 21:06:31:873_0
- RFN: 1792
- Chip: 27648
- Event: Send
- PCO: Dc
- Message: RRC_DataReq
- Source: ts_GMM_Authentication LINE 2
- Message Structure:
RRC_DataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[-1] = -
. (SapId)sapId[1] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. AUTHENTICATIONANDCIPHERINGREQUEST
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)gMMProtocolDiscriminator[4] = '1000'B
. . (MsgType)msgType[8] = '00010010'B
. . IMEISVRequest
. . . (B1)spare1[1] = '0'B
. . . (B3)value[3] = '000'B
. . CiphAlgorithm
. . . (B1)spare1[1] = '0'B
. . . (B3)algorithm[3] = '001'B
. . AC_ReferenceNumber
. . . (B4)value[4] = '0011'B
. . ForceToStandby
. . . (B1)spare[1] = '0'B
. . . (B3)value[3] = '000'B
. . AuthenticationParamterRAND
. . . (IEI8)iei[8] = '00100001'B
. . . (BitStringType)randValue[128] = '01010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101'B
. . CiphKeySeqNum_tv
. . . (IEI4)iei[4] = '1000'B
. . . (B1)spare1[1] = '0'B
. . . (KeySeq)keySeq[3] = '000'B
. . GMM_AUTN
. . . (IEI8)iei[8] = '00101000'B
. . . (Length)iel[1] = '10'O
. . . (BitStringType)aUTN[128] = '01010110010100010101000001010011010100100101110100000000000000000101010101010100010101110101011001010001010100000101001101010010'B
- Constraint:
ca_PS_DataReq
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 08 12 01 30 21 55 55 55 55 55 55 55 55 55 55 55 55 55 55 55 55 80 28 10 56 51 50 53 52 5d 00 00 55 54 57 56 51 50 53 52

- No.: 1269
- Timestamp: 21:06:32:531_0
- RFN: 1858
- Chip: 21248
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_GMM_Authentication LINE 7
- Message Structure:
RRC_DataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. (START_Value)start[0] = -
. AUTHENTICATIONANDCIPHERINGRESPONSE
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)gMMProtocolDiscriminator[4] = '1000'B
. . (MsgType)msgType[8] = '00010011'B
. . (B4)spare4[4] = '0000'B
. . AC_ReferenceNumber
. . . (B4)value[4] = '0011'B
. . AuthRsp_tv
. . . (IEI8)iei[8] = '00100010'B
. . . (BitStringType)value[32] = '01010101010101000101011101010110'B
. . GMM_MS_Identity
. . AuthRspExt
- Constraint:
car_PS_UplinkDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 08 13 03 22 55 54 57 56

- No.: 1272
- Timestamp: 21:06:32:534_1
- RFN: 1858
- Chip: 29952
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_GMM_Authentication LINE 10
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1309
- Timestamp: 21:06:32:546_0
- RFN: 1860
- Chip: 2560
- Event: Send
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_REQ
- Source: ts_SS_DownloadSecurityKey:lt_DownloadKeyCRLC LINE 1
- Message Structure:
CRLC_SecurityMode_Config_REQ
. (IntegerType)cellId = -1
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity = 1
. . (BitStringType)startValue[20] = "00000000000000000000"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = '01010111010101100101000101010000010100110101001001011101010111000101111101011110010110010101100001011011010110100101010101010100'B
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CRLC_SecurityModeCfgReq
- BinaryMessage:
30 21 02 01 ff 30 1c 0a 01 01 03 04 04 00 00 00 03 11 00 57 56 51 50 53 52 5d 5c 5f 5e 59 58 5b 5a 55 54

- No.: 1310
- Timestamp: 21:06:32:548_0
- RFN: 1860
- Chip: 9472
- Event: Receive
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_CNF
- Source: ts_SS_DownloadSecurityKey:lt_DownloadKeyCRLC LINE 2
- Message Structure:
CRLC_SecurityMode_Config_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1317
- Timestamp: 21:06:32:552_0
- RFN: 1860
- Chip: 22016
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 1
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
. (IntegerType)count_I_LSB_UL = -
. (IntegerType)count_I_LSB_DL = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 00 02 01 00 02 01 00

- No.: 1318
- Timestamp: 21:06:32:554_0
- RFN: 1860
- Chip: 29952
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 2
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 00 02 01 00

- No.: 1319
- Timestamp: 21:06:32:555_0
- RFN: 1860
- Chip: 37120
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 3
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. (IntegerType)count_I_LSB_UL = -
. (IntegerType)count_I_LSB_DL = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 01 02 01 00

- No.: 1320
- Timestamp: 21:06:32:557_0
- RFN: 1861
- Chip: 5632
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 4
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 1321
- Timestamp: 21:06:32:559_0
- RFN: 1861
- Chip: 12800
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 5
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. (IntegerType)count_I_LSB_UL = -
. (IntegerType)count_I_LSB_DL = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 02 02 01 00

- No.: 1322
- Timestamp: 21:06:32:561_0
- RFN: 1861
- Chip: 20480
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 6
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 1323
- Timestamp: 21:06:32:563_0
- RFN: 1861
- Chip: 27392
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 7
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
. (IntegerType)count_I_LSB_UL = -
. (IntegerType)count_I_LSB_DL = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 03 02 01 00

- No.: 1324
- Timestamp: 21:06:32:565_0
- RFN: 1861
- Chip: 34816
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 8
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 1325
- Timestamp: 21:06:32:567_0
- RFN: 1862
- Chip: 3584
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 9
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
. (IntegerType)count_I_LSB_UL = -
. (IntegerType)count_I_LSB_DL = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 04 02 01 00

- No.: 1326
- Timestamp: 21:06:32:568_0
- RFN: 1862
- Chip: 10496
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 10
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 1330
- Timestamp: 21:06:32:571_0
- RFN: 1862
- Chip: 21760
- Event: Send
- PCO: CRLC
- Message: CRLC_Integrity_Activate_REQ
- Source: ts_CRLC_DL_Integrity LINE 1
- Message Structure:
CRLC_Integrity_Activate_REQ
. (IntegerType)cellId = -1
. (CN_DomainIdentity)cn_DomainIdentity = 1
. IntegrityActivationInfo
. . IntegrityProtectionModeInfo
. . . IntegrityProtectionModeCommand
. . . . startIntegrityProtection
. . . . . (BitStringType)integrityProtInitNumber[32] = "00000000000000000000000000000001"
. . . (IntegrityProtectionAlgorithm)integrityProtectionAlgorithm = 0
- Constraint:
ca_CRLC_DL_IntegrityActivateReq
- BinaryMessage:
30 15 02 01 ff 0a 01 01 30 0d 30 30 07 03 05 00 00 00 00 01 0a 01 00

- No.: 1331
- Timestamp: 21:06:32:573_0
- RFN: 1862
- Chip: 28160
- Event: Receive
- PCO: CRLC
- Message: CRLC_Integrity_Activate_CNF
- Source: ts_CRLC_DL_Integrity LINE 2
- Message Structure:
CRLC_Integrity_Activate_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_IntegrityActivateCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1338
- Timestamp: 21:06:32:577_0
- RFN: 1863
- Chip: 4864
- Event: Send
- PCO: CRLC
- Message: CRLC_Integrity_Activate_REQ
- Source: ts_RB2_UL_IntegrityActivate LINE 1
- Message Structure:
CRLC_Integrity_Activate_REQ
. (IntegerType)cellId = -1
. (CN_DomainIdentity)cn_DomainIdentity = 1
. IntegrityActivationInfo
. . IntegrityProtActivationInfoList
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity = 2
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
- Constraint:
ca_CRLC_UL_IntegrityActivateReq
- BinaryMessage:
30 10 02 01 ff 0a 01 01 30 08 30 06 02 01 02 02 01 00

- No.: 1339
- Timestamp: 21:06:32:578_0
- RFN: 1863
- Chip: 10752
- Event: Receive
- PCO: CRLC
- Message: CRLC_Integrity_Activate_CNF
- Source: ts_RB2_UL_IntegrityActivate LINE 2
- Message Structure:
CRLC_Integrity_Activate_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_IntegrityActivateCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1345
- Timestamp: 21:06:32:585_0
- RFN: 1863
- Chip: 35072
- Event: Send
- PCO: AM
- Message: RLC_AM_DATA_REQ
- Source: ts_RRC_Security:lt_SendSecurityModeCommand LINE 7
- Message Structure:
RLC_AM_DATA_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. AmConfirmationRequest
. aM_message
. . DL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00000000000000000000000000000000"
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . DL_DCCH_MessageType
. . . . SecurityModeCommand
. . . . . r3
. . . . . . SecurityModeCommand_r3_IEs
. . . . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . . . SecurityCapability
. . . . . . . . (BitStringType)cipheringAlgorithmCap[16] = '0000000000000011'B
. . . . . . . . (BitStringType)integrityProtectionAlgorithmCap[16] = '0000000000000010'B
. . . . . . . CipheringModeInfo
. . . . . . . IntegrityProtectionModeInfo
. . . . . . . . IntegrityProtectionModeCommand
. . . . . . . . . startIntegrityProtection
. . . . . . . . . . (BitStringType)integrityProtInitNumber[32] = "00000000000000000000000000000001"
. . . . . . . . (IntegrityProtectionAlgorithm)integrityProtectionAlgorithm = 0
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity = 1
. . . . . . . InterRAT_UE_SecurityCapList
. . . . . . laterNonCriticalExtensions
- Constraint:
cas_RRC_SecModeCmd
- BinaryMessage:
30 17 02 01 ff 02 01 02 05 00 80 00 00 00 04 04 00 01 80 01 40 00 00 00 30

- No.: 1351
- Timestamp: 21:06:32:720_0
- RFN: 1877
- Chip: 13312
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_IND
- Source: ts_RRC_Security:lt_StartSecurity_UE LINE 8
- Message Structure:
RLC_AM_DATA_IND
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. IntegrityResult
. . (IntegrityStatus)integrityUsed = 0
. aM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "10000001100000001110110111011101"
. . . . (IntegerType)rrc_MessageSequenceNumber = 1
. . . UL_DCCH_MessageType
. . . . SecurityModeComplete
. . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . IntegrityProtActivationInfo
. . . . . . RRC_MessageSequenceNumberList
. . . . . . . (IntegerType)_elem = 0
. . . . . . . (IntegerType)_elem = 0
. . . . . . . (IntegerType)_elem = 0
. . . . . . . (IntegerType)_elem = 0
. . . . . . . (IntegerType)_elem = 0
. . . . . laterNonCriticalExtensions
. . . . . . (BitStringType)securityModeComplete_r3_add_ext = 0
. . . . . . nonCriticalExtensions
- Constraint:
car_RRC_SecModeCmpl
- BinaryMessage:
30 12 02 01 ff 02 01 02 0a 01 00 c0 c0 76 ee 8d 21 00 00 00

- No.: 1352
- Timestamp: 21:06:32:721_0
- RFN: 1877
- Chip: 17408
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_Security:lt_StartSecurity_UE LINE 8
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1354
- Timestamp: 21:06:32:725_0
- RFN: 1877
- Chip: 33792
- Event: Send
- PCO: CRLC
- Message: CRLC_Integrity_Activate_REQ
- Source: ts_CRLC_UL_Integrity LINE 1
- Message Structure:
CRLC_Integrity_Activate_REQ
. (IntegerType)cellId = -1
. (CN_DomainIdentity)cn_DomainIdentity = 1
. IntegrityActivationInfo
. . IntegrityProtActivationInfoList
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity = 0
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity = 1
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity = 3
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity = 4
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
- Constraint:
ca_CRLC_UL_IntegrityActivateReq
- BinaryMessage:
30 28 02 01 ff 0a 01 01 30 20 30 06 02 01 00 02 01 00 30 06 02 01 01 02 01 00 30 06 02 01 03 02 01 00 30 06 02 01 04 02 01 00

- No.: 1355
- Timestamp: 21:06:32:727_0
- RFN: 1878
- Chip: 2560
- Event: Receive
- PCO: CRLC
- Message: CRLC_Integrity_Activate_CNF
- Source: ts_CRLC_UL_Integrity LINE 2
- Message Structure:
CRLC_Integrity_Activate_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_IntegrityActivateCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1365
- Timestamp: 21:06:32:735_0
- RFN: 1878
- Chip: 32000
- Event: Send
- PCO: Dc
- Message: RRC_DataReq
- Source: ts_GMM_IdleUpdated:lt_AttachAccept LINE 12
- Message Structure:
RRC_DataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[-1] = -
. (SapId)sapId[1] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. ATTACHACCEPT
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)gMMProtocolDiscriminator[4] = '1000'B
. . (MsgType)msgType[8] = '00000010'B
. . ForceToStandby
. . . (B1)spare[1] = '0'B
. . . (B3)value[3] = '000'B
. . AttachResult
. . . (B1)spare[1] = '0'B
. . . (B3)result[3] = '001'B
. . GPRS_Timer_v
. . . (B3)unit[3] = '111'B
. . . (B5)value[5] = '00000'B
. . (B4)spare[4] = '0000'B
. . RadioPriority_v
. . . (B1)spare[1] = '0'B
. . . (B3)value[3] = '100'B
. . RAI_v
. . . (OctetStringType)plmn[3] = '00F110'O
. . . (OctetStringType)lac[2] = '0001'O
. . . (OctetStringType)rac[1] = '05'O
. . PTMSI_Signature
. . . (IEI8)iei[8] = '00011001'B
. . . (OctetStringType)value[3] = 'AB1234'O
. . GPRS_Timer
. . GMM_MS_IdentityPTMSI
. . . (IEI8)iei[8] = '00011000'B
. . . (Length)iel[1] = '05'O
. . . (B4)iDigit1[4] = '1111'B
. . . (B1)oddEvenInd[1] = '0'B
. . . (B3)typeOfId[3] = '100'B
. . . (OctetStringType)otherDigits[-1] = '12345678'O
. . GMM_MS_Identity
. . GMM_Cause
. . GPRS_Timer
. . CellNotification
. . PLMN_List
- Constraint:
ca_PS_DataReq
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 08 02 01 e0 04 00 f1 10 00 01 05 19 ab 12 34 18 05 f4 12 34 56 78

- No.: 1369
- Timestamp: 21:06:32:867_0
- RFN: 1892
- Chip: 5120
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_GMM_IdleUpdated:lt_AttachAccept LINE 13
- Message Structure:
RRC_DataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. (START_Value)start[0] = -
. ATTACHCOMPLETE
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)gMMProtocolDiscriminator[4] = '1000'B
. . (MsgType)msgType[8] = '00000011'B
- Constraint:
car_PS_UplinkDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 08 03

- No.: 1380
- Timestamp: 21:06:32:871_0
- RFN: 1892
- Chip: 18432
- Event: Start Timer
- Source: ts_RRC_Delay LINE 1
- Message Structure:
no details available
- Constraint:
t_Dly (1000 Ms)
- BinaryMessage:

- No.: 1384
- Timestamp: 21:06:33:858_0
- RFN: 1991
- Chip: 9728
- Event: Timeout
- Source: ts_RRC_Delay LINE 2
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 1389
- Timestamp: 21:06:33:863_0
- RFN: 1991
- Chip: 30208
- Event: Send
- PCO: UM
- Message: RLC_UM_DATA_REQ
- Source: ts_RRC_ConnRel:lt_Send_RRC_ConnectionRelease LINE 3
- Message Structure:
RLC_UM_DATA_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. uM_message
. . DL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00000000000000000000000000000000"
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . DL_DCCH_MessageType
. . . . RRCConnectionRelease
. . . . . r3
. . . . . . RRCConnectionRelease_r3_IEs
. . . . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . . . (IntegerType)n_308 = 1
. . . . . . . (ReleaseCause)releaseCause = 0
. . . . . . . Rplmn_Information
. . . . . . laterNonCriticalExtensions
. (BooleanType)specialLI = FALSE
- Constraint:
cas_RRC_ConnRelDCCH
- BinaryMessage:
30 10 02 01 ff 02 01 01 80 00 00 00 03 c8 00 01 01 00

- No.: 1393
- Timestamp: 21:06:33:989_0
- RFN: 2004
- Chip: 10240
- Event: Receive
- PCO: UM
- Message: RLC_UM_DATA_IND
- Source: ts_RRC_ConnRel:lt_Send_RRC_ConnectionRelease LINE 4
- Message Structure:
RLC_UM_DATA_IND
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. IntegrityResult
. uM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "10101101101011101001000000111001"
. . . . (IntegerType)rrc_MessageSequenceNumber = 1
. . . UL_DCCH_MessageType
. . . . RRCConnectionReleaseComplete
. . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . FailureCauseWithProtErr
. . . . . laterNonCriticalExtensions
. . . . . . (BitStringType)rrcConnectionReleaseComplete_r3_add_ext = 0
. . . . . . nonCriticalExtensions
- Constraint:
car_RRC_ConnRelCmplUM
- BinaryMessage:
30 0c 02 01 ff 02 01 01 d6 d7 48 1c 8c 40

- No.: 1394
- Timestamp: 21:06:33:990_0
- RFN: 2004
- Chip: 13824
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ConnRel:lt_Send_RRC_ConnectionRelease LINE 4
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1397
- Timestamp: 21:06:33:991_1
- RFN: 2004
- Chip: 18688
- Event: Start Timer
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 1
- Message Structure:
no details available
- Constraint:
t_Dly (5000 Ms)
- BinaryMessage:

- No.: 1401
- Timestamp: 21:06:34:138_0
- RFN: 2019
- Chip: 8192
- Event: Receive
- PCO: UM
- Message: RLC_UM_DATA_IND
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 4
- Message Structure:
RLC_UM_DATA_IND
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. IntegrityResult
. uM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00011100010101000111110101101001"
. . . . (IntegerType)rrc_MessageSequenceNumber = 2
. . . UL_DCCH_MessageType
. . . . RRCConnectionReleaseComplete
. . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . FailureCauseWithProtErr
. . . . . laterNonCriticalExtensions
. . . . . . (BitStringType)rrcConnectionReleaseComplete_r3_add_ext = 0
. . . . . . nonCriticalExtensions
- Constraint:
car_RRC_ConnRelCmplUM
- BinaryMessage:
30 0c 02 01 ff 02 01 01 8e 2a 3e b4 94 40

- No.: 1402
- Timestamp: 21:06:34:139_0
- RFN: 2019
- Chip: 12288
- Event: Cancel Timer
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 4
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 1403
- Timestamp: 21:06:34:139_1
- RFN: 2019
- Chip: 13056
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 4
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1409
- Timestamp: 21:06:34:143_0
- RFN: 2019
- Chip: 26880
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 01 0a 01 00 05 00

- No.: 1413
- Timestamp: 21:06:34:150_0
- RFN: 2020
- Chip: 15616
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 1416
- Timestamp: 21:06:34:153_0
- RFN: 2020
- Chip: 27136
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 02 0a 01 00 05 00

- No.: 1420
- Timestamp: 21:06:34:160_0
- RFN: 2021
- Chip: 17152
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 1423
- Timestamp: 21:06:34:163_0
- RFN: 2021
- Chip: 28160
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 03 0a 01 00 05 00

- No.: 1427
- Timestamp: 21:06:34:170_0
- RFN: 2022
- Chip: 17152
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 1430
- Timestamp: 21:06:34:173_0
- RFN: 2022
- Chip: 27904
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 04 0a 01 00 05 00

- No.: 1434
- Timestamp: 21:06:34:184_0
- RFN: 2023
- Chip: 31488
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 1437
- Timestamp: 21:06:34:191_0
- RFN: 2024
- Chip: 20736
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 136
. . . . . UL_RLC_Mode
. . . . . . UL_UM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (NoExplicitDiscard)timerBasedNoExplicit = 9
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = 1
. . . . (IntegerType)dLlogicalChannelIdentity = 1
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_UM_Info
- BinaryMessage:
30 22 02 01 ff 02 01 01 0a 01 00 30 17 30 0d 05 00 30 09 02 02 00 88 30 03 0a 01 09 30 06 02 01 01 02 01 01

- No.: 1441
- Timestamp: 21:06:34:199_0
- RFN: 2025
- Chip: 11776
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 1442
- Timestamp: 21:06:34:207_0
- RFN: 2026
- Chip: 5120
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 3
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . (TimerEPC)timerEPC = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . (TimerRST)timerRST = 9
. . . . . . . (MaxRST)max_RST = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = 2
. . . . (IntegerType)dLlogicalChannelIdentity = 2
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 02 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 27 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 02 02 01 02

- No.: 1446
- Timestamp: 21:06:34:224_0
- RFN: 2027
- Chip: 33024
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 4
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 1447
- Timestamp: 21:06:34:233_0
- RFN: 2028
- Chip: 27904
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 5
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . (TimerEPC)timerEPC = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . (TimerRST)timerRST = 9
. . . . . . . (MaxRST)max_RST = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = 3
. . . . (IntegerType)dLlogicalChannelIdentity = 3
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 03 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 27 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 03 02 01 03

- No.: 1451
- Timestamp: 21:06:34:253_0
- RFN: 2030
- Chip: 29184
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 6
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 1452
- Timestamp: 21:06:34:262_0
- RFN: 2031
- Chip: 26368
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 7
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . (TimerEPC)timerEPC = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . (TimerRST)timerRST = 9
. . . . . . . (MaxRST)max_RST = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = 4
. . . . (IntegerType)dLlogicalChannelIdentity = 4
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 04 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 27 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 04 02 01 04

- No.: 1456
- Timestamp: 21:06:34:284_0
- RFN: 2033
- Chip: 30464
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 8
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 1498
- Timestamp: 21:06:34:299_0
- RFN: 2035
- Chip: 8960
- Event: Start Timer
- Source: ts_RRC_Delay LINE 1
- Message Structure:
no details available
- Constraint:
t_Dly (5000 Ms)
- BinaryMessage:

- No.: 1500
- Timestamp: 21:06:34:301_0
- RFN: 2035
- Chip: 19712
- Event: Receive
- PCO: CPHY
- Message: CPHY_Out_of_Sync_IND
- Source: RRC_Def1 LINE 15
- Message Structure:
CPHY_Out_of_Sync_IND
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_OutOfSyncInd
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 1501
- Timestamp: 21:06:34:302_0
- RFN: 2035
- Chip: 21760
- Event: Cancel Timer
- Source: RRC_Def1 LINE 15
- Message Structure:
no details available
- Constraint:
t_T312
- BinaryMessage:

- No.: 1502
- Timestamp: 21:06:34:303_0
- RFN: 2035
- Chip: 25088
- Event: Default
- Source: RRC_Def1 LINE 0
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1503
- Timestamp: 21:06:34:303_1
- RFN: 2035
- Chip: 25856
- Event: Default
- Source: ts_RRC_Delay LINE 2
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1508
- Timestamp: 21:06:39:288_0
- RFN: 2534
- Chip: 11008
- Event: Timeout
- Source: ts_RRC_Delay LINE 2
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 1521
- Timestamp: 21:06:39:301_0
- RFN: 2535
- Chip: 16384
- Event: Send
- PCO: CMAC
- Message: CMAC_PAGING_Config_REQ
- Source: ts_CMAC_Pag1_Cfg LINE 4
- Message Structure:
CMAC_PAGING_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 5
. (RatType)ratType = 0
. CmacPagingConfigReq
. . pI_BitMapInfo
. . . (BitStringType)e18[18] = '010000000000000000'B
. . (IntegerType)dRX_CycleLength = 7
. . IMSI_GSM_MAP
. . . (IntegerType)_elem = 0
. . . (IntegerType)_elem = 0
. . . (IntegerType)_elem = 1
. . . (IntegerType)_elem = 0
. . . (IntegerType)_elem = 1
. . . (IntegerType)_elem = 0
. . . (IntegerType)_elem = 1
. . . (IntegerType)_elem = 2
. . . (IntegerType)_elem = 3
. . . (IntegerType)_elem = 4
. . . (IntegerType)_elem = 5
. . . (IntegerType)_elem = 6
. . . (IntegerType)_elem = 0
. . . (IntegerType)_elem = 6
. . . (IntegerType)_elem = 3
. . (BooleanType)t_pich_T_sccpch = FALSE
- Constraint:
ca_CMAC_PagingCfgReq
- BinaryMessage:
30 46 02 01 00 02 01 05 0a 01 00 30 3b 03 04 06 40 00 00 02 01 07 30 2d 02 01 00 02 01 00 02 01 01 02 01 00 02 01 01 02 01 00 02 01 01 02 01 02 02 01 03 02 01 04 02 01 05 02 01 06 02 01 00 02 01 06 02 01 03 01 01 00

- No.: 1525
- Timestamp: 21:06:39:308_0
- RFN: 2536
- Chip: 5376
- Event: Receive
- PCO: CMAC
- Message: CMAC_PAGING_Config_CNF
- Source: ts_CMAC_Pag1_Cfg LINE 5
- Message Structure:
CMAC_PAGING_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 5
- Constraint:
ca_CMAC_PagingCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 05

- No.: 1527
- Timestamp: 21:06:39:316_0
- RFN: 2537
- Chip: 768
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_RRC_ConnEst_DCH_MT_PTMSI LINE 5
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -2
. tM_message
. . PCCH_Message
. . . PCCH_MessageType
. . . . PagingType1
. . . . . PagingRecordList
. . . . . . PagingRecord
. . . . . . . cn_Identity
. . . . . . . . (PagingCause)pagingCause = 2
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = 1
. . . . . . . . CN_PagedUE_Identity
. . . . . . . . . (BitStringType)p_TMSI_GSM_MAP[32] = "00010010001101000101011001111000"
. . . . . BCCH_ModificationInfo
. . . . . laterNonCriticalExtensions
- Constraint:
cas_PagingType1
- BinaryMessage:
30 0c 02 01 00 02 01 fe 40 54 24 68 ac f0

- No.: 1531
- Timestamp: 21:06:40:478_0
- RFN: 2653
- Chip: 8192
- Event: Receive
- PCO: TM
- Message: RLC_TR_DATA_IND
- Source: ts_RRC_ConnEst_DCH_MT_PTMSI LINE 6
- Message Structure:
RLC_TR_DATA_IND
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
. tM_message
. . UL_CCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode = 0
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . UL_CCCH_MessageType
. . . . RRCConnectionRequest
. . . . . InitialUE_Identity
. . . . . . TMSI_and_LAI_GSM_MAP
. . . . . . . (BitStringType)tmsi[32] = "00010010001101000101011001111000"
. . . . . . . LAI
. . . . . . . . PLMN_Identity
. . . . . . . . . MCC
. . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . (IntegerType)_elem = 1
. . . . . . . . . MNC
. . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . (IntegerType)_elem = 1
. . . . . . . . (BitStringType)lac[16] = '0000000000000001'B
. . . . . (EstablishmentCause)establishmentCause = 7
. . . . . (ProtocolErrorIndicator)protocolErrorIndicator = 0
. . . . . MeasuredResultsOnRACH
. . . . . . currentCell
. . . . . . . modeSpecificInfo
. . . . . . . . fdd
. . . . . . . . . measurementQuantity
. . . . . . . . . . (IntegerType)cpich_Ec_N0 = 0
. . . . . v3d0NonCriticalExtensions
. . . . . . RRCConnectionRequest_v3d0ext_IEs
. . . . . . . (BitStringType)uESpecificBehaviourInformation1idle = 0
. . . . . . nonCriticalExtensions
- Constraint:
car_RRC_ConnReq
- BinaryMessage:
30 11 02 01 00 02 01 00 21 12 34 56 78 00 10 08 00 09 c0

- No.: 1532
- Timestamp: 21:06:40:537_0
- RFN: 2659
- Chip: 7168
- Event: Send
- PCO: UM
- Message: RLC_UM_DATA_REQ
- Source: ts_RRC_ConnEst_DCH_MT_PTMSI LINE 7
- Message Structure:
RLC_UM_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
. uM_message
. . DL_CCCH_Message
. . . IntegrityCheckInfo
. . . DL_CCCH_MessageType
. . . . RRCConnectionSetup
. . . . . r3
. . . . . . RRCConnectionSetup_r3_IEs
. . . . . . . InitialUE_Identity
. . . . . . . . TMSI_and_LAI_GSM_MAP
. . . . . . . . . (BitStringType)tmsi[32] = "00010010001101000101011001111000"
. . . . . . . . . LAI
. . . . . . . . . . PLMN_Identity
. . . . . . . . . . . MCC
. . . . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . . . (IntegerType)_elem = 1
. . . . . . . . . . . MNC
. . . . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . . . (IntegerType)_elem = 1
. . . . . . . . . . (BitStringType)lac[16] = '0000000000000001'B
. . . . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . . . (IntegerType)activationTime = -
. . . . . . . U_RNTI
. . . . . . . . (BitStringType)srnc_Identity[12] = "000000000001"
. . . . . . . . (BitStringType)s_RNTI[20] = "00000000000000000001"
. . . . . . . (BitStringType)new_c_RNTI[16] = -
. . . . . . . (RRC_StateIndicator)rrc_StateIndicator = 0
. . . . . . . (IntegerType)utran_DRX_CycleLengthCoeff = 9
. . . . . . . CapabilityUpdateRequirement
. . . . . . . . (BooleanType)ue_RadioCapabilityFDDUpdateRequirement = TRUE
. . . . . . . . (BooleanType)ue_RadioCapabilityTDDUpdateRequirement = FALSE
. . . . . . . . SystemSpecificCapUpdateReqList
. . . . . . . . . (SystemSpecificCapUpdateReq)_elem = 0
. . . . . . . SRB_InformationSetupList2
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_UM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 1
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 1
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . . . . . . . (TimerRST)timerRST = 9
. . . . . . . . . . . . . (MaxRST)max_RST = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 2
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 2
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . . . . . . . (TimerRST)timerRST = 9
. . . . . . . . . . . . . (MaxRST)max_RST = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 3
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 3
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . . . . . . . (TimerRST)timerRST = 9
. . . . . . . . . . . . . (MaxRST)max_RST = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 4
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 4
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . UL_CommonTransChInfo
. . . . . . . . TFC_Subset
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . TFCS
. . . . . . . . . . . ExplicitTFCS_Configuration
. . . . . . . . . . . . TFCS_ReconfAdd
. . . . . . . . . . . . . ctfcSize
. . . . . . . . . . . . . . ctfc2Bit
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . . . . . . . (IntegerType)ctfc2 = 0
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . . . . . . . (IntegerType)ctfc2 = 1
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 11
. . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . UL_AddReconfTransChInfoList
. . . . . . . . UL_AddReconfTransChInformation
. . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType = 0
. . . . . . . . . (IntegerType)transportChannelIdentity = 5
. . . . . . . . . TransportFormatSet
. . . . . . . . . . DedicatedTransChTFS
. . . . . . . . . . . tti
. . . . . . . . . . . . DedicatedDynamicTF_InfoList
. . . . . . . . . . . . . DedicatedDynamicTF_Info
. . . . . . . . . . . . . . rlc_Size
. . . . . . . . . . . . . . . BitModeRLC_SizeInfo
. . . . . . . . . . . . . . . . sizeType2
. . . . . . . . . . . . . . . . . (IntegerType)part1 = 2
. . . . . . . . . . . . . . . . . (IntegerType)part2 = -
. . . . . . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . LogicalChannelList
. . . . . . . . . . . SemistaticTF_Information
. . . . . . . . . . . . ChannelCodingType
. . . . . . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . . . . . (IntegerType)rateMatchingAttribute = 192
. . . . . . . . . . . . (CRC_Size)crc_Size = 3
. . . . . . . DL_CommonTransChInfo
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . dl_Parameters
. . . . . . . DL_AddReconfTransChInfoList
. . . . . . . . DL_AddReconfTransChInformation
. . . . . . . . . (DL_TrCH_Type)dl_TransportChannelType = 0
. . . . . . . . . (IntegerType)dl_transportChannelIdentity = 10
. . . . . . . . . tfs_SignallingMode
. . . . . . . . . . UL_TransportChannelIdentity
. . . . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType = 0
. . . . . . . . . . . (IntegerType)ul_TransportChannelIdentity = 5
. . . . . . . . . QualityTarget
. . . . . . . . . . (IntegerType)bler_QualityValue = -20
. . . . . . . . . TM_SignallingInfo
. . . . . . . FrequencyInfo
. . . . . . . (IntegerType)maxAllowedUL_TX_Power = -
. . . . . . . UL_ChannelRequirement
. . . . . . . . UL_DPCH_Info
. . . . . . . . . UL_DPCH_PowerControlInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (IntegerType)dpcch_PowerOffset = -40
. . . . . . . . . . . (IntegerType)pc_Preamble = 1
. . . . . . . . . . . (IntegerType)sRB_delay = 7
. . . . . . . . . . . PowerControlAlgorithm
. . . . . . . . . . . . (IntegerType)algorithm1 = 1
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (ScramblingCodeType)scramblingCodeType = 1
. . . . . . . . . . . (IntegerType)scramblingCode = 0
. . . . . . . . . . . (IntegerType)numberOfDPDCH = -
. . . . . . . . . . . (SpreadingFactor)spreadingFactor = 4
. . . . . . . . . . . (BooleanType)tfci_Existence = TRUE
. . . . . . . . . . . (IntegerType)numberOfFBI_Bits = -
. . . . . . . . . . . (PuncturingLimit)puncturingLimit = 15
. . . . . . . DL_CommonInformation
. . . . . . . . DL_DPCH_InfoCommon
. . . . . . . . . cfnHandling
. . . . . . . . . . initialise
. . . . . . . . . . . (IntegerType)cfntargetsfnframeoffset = -
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . DL_DPCH_PowerControlInfo
. . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . (DPC_Mode)dpc_Mode = 0
. . . . . . . . . . . (IntegerType)powerOffsetPilot_pdpdch = 0
. . . . . . . . . . . Dl_rate_matching_restriction
. . . . . . . . . . . SF512_AndPilot
. . . . . . . . . . . . (PilotBits128)sfd128 = 0
. . . . . . . . . . . (PositionFixedOrFlexible)positionFixedOrFlexible = 0
. . . . . . . . . . . (BooleanType)tfci_Existence = FALSE
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . (IntegerType)defaultDPCH_OffsetValue = 0
. . . . . . . . . . DPCH_CompressedModeInfo
. . . . . . . . . . (TX_DiversityMode)tx_DiversityMode = 0
. . . . . . . . . . SSDT_Information
. . . . . . . DL_InformationPerRL_List
. . . . . . . . DL_InformationPerRL
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . PrimaryCPICH_Info
. . . . . . . . . . . . (IntegerType)primaryScramblingCode = 100
. . . . . . . . . . . PDSCH_SHO_DCH_Info
. . . . . . . . . . . PDSCH_CodeMapping
. . . . . . . . . DL_DPCH_InfoPerRL
. . . . . . . . . . fdd
. . . . . . . . . . . (PCPICH_UsageForChannelEst)pCPICH_UsageForChannelEst = 0
. . . . . . . . . . . (IntegerType)dpch_FrameOffset = 0
. . . . . . . . . . . SecondaryCPICH_Info
. . . . . . . . . . . DL_ChannelisationCodeList
. . . . . . . . . . . . DL_ChannelisationCode
. . . . . . . . . . . . . (IntegerType)secondaryScramblingCode = 1
. . . . . . . . . . . . . SF512_AndCodeNumber
. . . . . . . . . . . . . . (IntegerType)sf128 = 0
. . . . . . . . . . . . . (ScramblingCodeChange)scramblingCodeChange = 1
. . . . . . . . . . . (IntegerType)tpc_CombinationIndex = 0
. . . . . . . . . . . (SSDT_CellIdentity)ssdt_CellIdentity = -
. . . . . . . . . . . (ClosedLoopTimingAdjMode)closedLoopTimingAdjMode = -
. . . . . . . . . SCCPCH_InfoForFACH
. . . . . . laterNonCriticalExtensions
. (BooleanType)specialLI = TRUE
- Constraint:
cas_RRC_ConnSetup
- BinaryMessage:
30 78 02 01 00 02 01 00 30 e7 22 46 8a cf 00 02 01 00 01 00 04 00 00 4d 82 69 3a 10 10 89 0d 42 00 02 81 9e 8e 46 c9 ce 7c 9c 4e 74 20 a5 12 3a 8c 00 15 13 3d 1c 8d 93 9c f9 38 9c e8 42 52 24 b5 28 00 4a 46 7a 39 1b 27 39 f2 71 39 d0 86 b4 49 ea 70 00 d4 c8 00 06 25 2b f0 02 00 08 82 23 bf 66 08 98 95 a5 47 a2 00 00 01 3f 90 0a 14 00 02 06 40 00 0c 28 08 01 01 ff

- No.: 1540
- Timestamp: 21:06:40:578_2
- RFN: 2663
- Chip: 7936
- Event: Start Timer
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 3
- Message Structure:
no details available
- Constraint:
t_WaitMS (13500 Ms)
- BinaryMessage:

- No.: 1545
- Timestamp: 21:06:40:813_0
- RFN: 2686
- Chip: 30720
- Event: Receive
- PCO: CPHY
- Message: CPHY_Sync_IND
- Source: RRC_Def1 LINE 13
- Message Structure:
CPHY_Sync_IND
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_SyncInd
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 1546
- Timestamp: 21:06:40:814_0
- RFN: 2686
- Chip: 32512
- Event: Cancel Timer
- Source: RRC_Def1 LINE 13
- Message Structure:
no details available
- Constraint:
t_T312
- BinaryMessage:

- No.: 1547
- Timestamp: 21:06:40:814_1
- RFN: 2686
- Chip: 34304
- Event: Default
- Source: RRC_Def1 LINE 0
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1548
- Timestamp: 21:06:40:815_0
- RFN: 2686
- Chip: 35072
- Event: Default
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1553
- Timestamp: 21:06:40:930_0
- RFN: 2698
- Chip: 13312
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_IND
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
RLC_AM_DATA_IND
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. IntegrityResult
. . (IntegrityStatus)integrityUsed = 0
. aM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode = 0
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . UL_DCCH_MessageType
. . . . RRCConnectionSetupComplete
. . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . STARTList
. . . . . . STARTSingle
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity = 1
. . . . . . . (BitStringType)start_Value[20] = "00000000000000000010"
. . . . . . STARTSingle
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity = 0
. . . . . . . (BitStringType)start_Value[20] = "00000000000000000010"
. . . . . UE_RadioAccessCapability
. . . . . . (AccessStratumReleaseIndicator)accessStratumReleaseIndicator = 0
. . . . . . PDCP_Capability
. . . . . . . (BooleanType)losslessSRNS_RelocationSupport = FALSE
. . . . . . . supportForRfc2507
. . . . . . RLC_Capability
. . . . . . . (TotalRLC_AM_BufferSize)totalRLC_AM_BufferSize = 2
. . . . . . . (MaximumRLC_WindowSize)maximumRLC_WindowSize = 0
. . . . . . . (MaximumAM_EntityNumberRLC_Cap)maximumAM_EntityNumber = 3
. . . . . . TransportChannelCapability
. . . . . . . DL_TransChCapability
. . . . . . . . (MaxNoBits)maxNoBitsReceived = 4
. . . . . . . . (MaxNoBits)maxConvCodeBitsReceived = 1
. . . . . . . . TurboSupport
. . . . . . . . . (MaxNoBits)supported = 4
. . . . . . . . (MaxSimultaneousTransChsDL)maxSimultaneousTransChs = 1
. . . . . . . . (IntegerType)maxSimultaneousCCTrCH_Count = 1
. . . . . . . . (MaxTransportBlocksDL)maxReceivedTransportBlocks = 2
. . . . . . . . (MaxNumberOfTFC_DL)maxNumberOfTFC = 4
. . . . . . . . (MaxNumberOfTF)maxNumberOfTF = 1
. . . . . . . UL_TransChCapability
. . . . . . . . (MaxNoBits)maxNoBitsTransmitted = 3
. . . . . . . . (MaxNoBits)maxConvCodeBitsTransmitted = 1
. . . . . . . . TurboSupport
. . . . . . . . . (MaxNoBits)supported = 3
. . . . . . . . (MaxSimultaneousTransChsUL)maxSimultaneousTransChs = 2
. . . . . . . . modeSpecificInfo
. . . . . . . . (MaxTransportBlocksUL)maxTransmittedBlocks = 2
. . . . . . . . (MaxNumberOfTFC_UL)maxNumberOfTFC = 3
. . . . . . . . (MaxNumberOfTF)maxNumberOfTF = 0
. . . . . . RF_Capability
. . . . . . . fddRF_Capability
. . . . . . . . (IntegerType)ue_PowerClass = 4
. . . . . . . . (TxRxFrequencySeparation)txRxFrequencySeparation = 0
. . . . . . . tddRF_Capability
. . . . . . . . (IntegerType)ue_PowerClass = 0
. . . . . . . . (RadioFrequencyBandTDDList)radioFrequencyTDDBandList = 0
. . . . . . . . (ChipRateCapability)chipRateCapability = 0
. . . . . . PhysicalChannelCapability
. . . . . . . fddPhysChCapability
. . . . . . . . DL_PhysChCapabilityFDD
. . . . . . . . . (IntegerType)maxNoDPCH_PDSCH_Codes = 3
. . . . . . . . . (MaxNoPhysChBitsReceived)maxNoPhysChBitsReceived = 6
. . . . . . . . . (BooleanType)supportForSF_512 = FALSE
. . . . . . . . . (BooleanType)supportOfPDSCH = FALSE
. . . . . . . . . SimultaneousSCCPCH_DPCH_Reception
. . . . . . . . UL_PhysChCapabilityFDD
. . . . . . . . . (MaxNoDPDCH_BitsTransmitted)maxNoDPDCH_BitsTransmitted = 2
. . . . . . . . . (BooleanType)supportOfPCPCH = FALSE
. . . . . . . tddPhysChCapability
. . . . . . . . DL_PhysChCapabilityTDD
. . . . . . . . . (IntegerType)maxTS_PerFrame = 0
. . . . . . . . . (IntegerType)maxPhysChPerFrame = 0
. . . . . . . . . (MinimumSF_DL)minimumSF = 0
. . . . . . . . . (BooleanType)supportOfPDSCH = FALSE
. . . . . . . . . (IntegerType)maxPhysChPerTS = 0
. . . . . . . . UL_PhysChCapabilityTDD
. . . . . . . . . (IntegerType)maxTS_PerFrame = 0
. . . . . . . . . (MaxPhysChPerTimeslot)maxPhysChPerTimeslot = 0
. . . . . . . . . (MinimumSF_UL)minimumSF = 0
. . . . . . . . . (BooleanType)supportOfPUSCH = FALSE
. . . . . . UE_MultiModeRAT_Capability
. . . . . . . MultiRAT_Capability
. . . . . . . . (BooleanType)supportOfGSM = TRUE
. . . . . . . . (BooleanType)supportOfMulticarrier = FALSE
. . . . . . . (MultiModeCapability)multiModeCapability = 1
. . . . . . SecurityCapability
. . . . . . . (BitStringType)cipheringAlgorithmCap[16] = '0000000000000011'B
. . . . . . . (BitStringType)integrityProtectionAlgorithmCap[16] = '0000000000000010'B
. . . . . . UE_Positioning_Capability
. . . . . . . (BooleanType)standaloneLocMethodsSupported = FALSE
. . . . . . . (BooleanType)ue_BasedOTDOA_Supported = FALSE
. . . . . . . (NetworkAssistedGPS_Supported)networkAssistedGPS_Supported = 3
. . . . . . . (BooleanType)supportForUE_GPS_TimingOfCellFrames = FALSE
. . . . . . . (BooleanType)supportForIPDL = FALSE
. . . . . . MeasurementCapability
. . . . . . . CompressedModeMeasCapability
. . . . . . . . (BooleanType)fdd_Measurements = TRUE
. . . . . . . . (BooleanType)tdd_Measurements = FALSE
. . . . . . . . GSM_Measurements
. . . . . . . . . (BooleanType)gsm900 = TRUE
. . . . . . . . . (BooleanType)dcs1800 = TRUE
. . . . . . . . . (BooleanType)gsm1900 = FALSE
. . . . . . . . (BooleanType)multiCarrierMeasurements = FALSE
. . . . . . . CompressedModeMeasCapability
. . . . . . . . (BooleanType)fdd_Measurements = TRUE
. . . . . . . . (BooleanType)tdd_Measurements = FALSE
. . . . . . . . GSM_Measurements
. . . . . . . . . (BooleanType)gsm900 = TRUE
. . . . . . . . . (BooleanType)dcs1800 = TRUE
. . . . . . . . . (BooleanType)gsm1900 = FALSE
. . . . . . . . (BooleanType)multiCarrierMeasurements = FALSE
. . . . . v370NonCriticalExtensions
. . . . . . RRCConnectionSetupComplete_v370ext
. . . . . . . UE_RadioAccessCapability_v370ext
. . . . . . v380NonCriticalExtensions
. . . . . . . RRCConnectionSetupComplete_v380ext_IEs
. . . . . . . . UE_RadioAccessCapability_v380ext
. . . . . . . . . UE_PositioningCapabilityExt_v380
. . . . . . . . . . (BooleanType)rx_tx_TimeDifferenceType2Capable = FALSE
. . . . . . . . DL_PhysChCapabilityFDD_v380ext
. . . . . . . . . (SupportOfDedicatedPilotsForChEstimation)supportOfDedicatedPilotsForChEstimation = 0
. . . . . . . v3a0NonCriticalExtensions
. . . . . . . . RRCConnectionSetupComplete_v3a0ext_IEs
. . . . . . . . . UE_RadioAccessCapability_v3a0ext
. . . . . . . . . . UE_PositioningCapabilityExt_v3a0
. . . . . . . . . . . (UE_PositioningCapabilityExt_v3a0_list_0)validity_CellPCH_UraPCH = 0
. . . . . . . . laterNonCriticalExtensions
. . . . . . . . . (BitStringType)rrcConnectionSetupComplete_r3_add_ext = 0
. . . . . . . . . nonCriticalExtensions
- Constraint:
car_RRC_ConnSetupCmpl
- BinaryMessage:
30 27 02 01 ff 02 01 02 0a 05 01 00 00 00 00 4a 0c 00 00 80 00 05 11 a0 d1 04 84 c6 68 46 2c 93 02 48 00 18 00 11 8f 8f 80

- No.: 1554
- Timestamp: 21:06:40:938_0
- RFN: 2699
- Chip: 6656
- Event: Cancel Timer
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
t_WaitMS
- BinaryMessage:

- No.: 1555
- Timestamp: 21:06:40:938_1
- RFN: 2699
- Chip: 7680
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1569
- Timestamp: 21:06:40:946_0
- RFN: 2700
- Chip: 1536
- Event: Send
- PCO: CMAC
- Message: CMAC_SecurityMode_Config_REQ
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 1
- Message Structure:
CMAC_SecurityMode_Config_REQ
. (IntegerType)cellId = 0
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity = 1
. . (BitStringType)startValue[20] = "00000000000000000010"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = -
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CMAC_SecurityModeCfgReq
- BinaryMessage:
30 0e 02 01 00 30 09 0a 01 01 03 04 04 00 00 20

- No.: 1570
- Timestamp: 21:06:40:948_0
- RFN: 2700
- Chip: 8448
- Event: Receive
- PCO: CMAC
- Message: CMAC_SecurityMode_Config_CNF
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 2
- Message Structure:
CMAC_SecurityMode_Config_CNF
. (IntegerType)cellId = 0
- Constraint:
ca_CMAC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 00

- No.: 1571
- Timestamp: 21:06:40:950_0
- RFN: 2700
- Chip: 15616
- Event: Send
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_REQ
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 3
- Message Structure:
CRLC_SecurityMode_Config_REQ
. (IntegerType)cellId = -1
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity = 1
. . (BitStringType)startValue[20] = "00000000000000000010"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = -
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CRLC_SecurityModeCfgReq
- BinaryMessage:
30 0e 02 01 ff 30 09 0a 01 01 03 04 04 00 00 20

- No.: 1572
- Timestamp: 21:06:40:952_0
- RFN: 2700
- Chip: 22272
- Event: Receive
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_CNF
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 4
- Message Structure:
CRLC_SecurityMode_Config_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1586
- Timestamp: 21:06:40:957_0
- RFN: 2701
- Chip: 4096
- Event: Send
- PCO: CMAC
- Message: CMAC_SecurityMode_Config_REQ
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 1
- Message Structure:
CMAC_SecurityMode_Config_REQ
. (IntegerType)cellId = 0
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity = 0
. . (BitStringType)startValue[20] = "00000000000000000010"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = -
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CMAC_SecurityModeCfgReq
- BinaryMessage:
30 0e 02 01 00 30 09 0a 01 00 03 04 04 00 00 20

- No.: 1587
- Timestamp: 21:06:40:959_0
- RFN: 2701
- Chip: 11008
- Event: Receive
- PCO: CMAC
- Message: CMAC_SecurityMode_Config_CNF
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 2
- Message Structure:
CMAC_SecurityMode_Config_CNF
. (IntegerType)cellId = 0
- Constraint:
ca_CMAC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 00

- No.: 1588
- Timestamp: 21:06:40:961_0
- RFN: 2701
- Chip: 18176
- Event: Send
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_REQ
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 3
- Message Structure:
CRLC_SecurityMode_Config_REQ
. (IntegerType)cellId = -1
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity = 0
. . (BitStringType)startValue[20] = "00000000000000000010"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = -
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CRLC_SecurityModeCfgReq
- BinaryMessage:
30 0e 02 01 ff 30 09 0a 01 00 03 04 04 00 00 20

- No.: 1589
- Timestamp: 21:06:40:962_0
- RFN: 2701
- Chip: 24576
- Event: Receive
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_CNF
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 4
- Message Structure:
CRLC_SecurityMode_Config_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1610
- Timestamp: 21:06:40:973_0
- RFN: 2702
- Chip: 25600
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: pr_GenericSetupProcedures:lt_ReceiveResponseToPaging LINE 2
- Message Structure:
RRC_DataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. (START_Value)start[20] = '00000000000000000010'B
. SERVICEREQUEST
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)gMMProtocolDiscriminator[4] = '1000'B
. . (MsgType)msgType[8] = '00001100'B
. . ServiceType_v
. . . (B1)spare1[1] = '0'B
. . . (B3)type[3] = '010'B
. . CiphKeySeqNum
. . . (B1)spare1[1] = '0'B
. . . (KeySeq)keySeq[3] = '000'B
. . MS_Identity_lv
. . . (Length)iel[1] = '05'O
. . . (B4)iDigit1[4] = '1111'B
. . . (B1)oddEvenInd[1] = '0'B
. . . (B3)typeOfId[3] = '100'B
. . . (OctetStringType)otherDigits[4] = '12345678'O
. . PDP_ContextStatus
. . . (IEI8)iei[8] = '00110010'B
. . . (Length)iel[1] = '02'O
. . . (BitStringType)nSAPI[16] = '0000000000000000'B
- Constraint:
car_PS_InitDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 03 04 04 00 00 20 08 0c 20 05 f4 12 34 56 78 32 02 00 00

- No.: 1644
- Timestamp: 21:06:40:986_0
- RFN: 2704
- Chip: 256
- Event: Send
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_REQ
- Source: ts_SS_DownloadSecurityKey:lt_DownloadKeyCRLC LINE 1
- Message Structure:
CRLC_SecurityMode_Config_REQ
. (IntegerType)cellId = -1
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity = 1
. . (BitStringType)startValue[20] = "00000000000000000010"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = '01010111010101100101000101010000010100110101001001011101010111000101111101011110010110010101100001011011010110100101010101010100'B
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CRLC_SecurityModeCfgReq
- BinaryMessage:
30 21 02 01 ff 30 1c 0a 01 01 03 04 04 00 00 20 03 11 00 57 56 51 50 53 52 5d 5c 5f 5e 59 58 5b 5a 55 54

- No.: 1645
- Timestamp: 21:06:40:988_0
- RFN: 2704
- Chip: 7680
- Event: Receive
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_CNF
- Source: ts_SS_DownloadSecurityKey:lt_DownloadKeyCRLC LINE 2
- Message Structure:
CRLC_SecurityMode_Config_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1652
- Timestamp: 21:06:40:991_0
- RFN: 2704
- Chip: 19712
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 1
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
. (IntegerType)count_I_LSB_UL = -
. (IntegerType)count_I_LSB_DL = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 00 02 01 00 02 01 00

- No.: 1653
- Timestamp: 21:06:40:993_0
- RFN: 2704
- Chip: 27136
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 2
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 00 02 01 00

- No.: 1654
- Timestamp: 21:06:40:995_0
- RFN: 2704
- Chip: 33792
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 3
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. (IntegerType)count_I_LSB_UL = -
. (IntegerType)count_I_LSB_DL = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 01 02 01 00

- No.: 1655
- Timestamp: 21:06:40:997_0
- RFN: 2705
- Chip: 3584
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 4
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 1656
- Timestamp: 21:06:40:999_0
- RFN: 2705
- Chip: 11264
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 5
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. (IntegerType)count_I_LSB_UL = -
. (IntegerType)count_I_LSB_DL = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 02 02 01 00

- No.: 1657
- Timestamp: 21:06:41:001_0
- RFN: 2705
- Chip: 18432
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 6
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 1658
- Timestamp: 21:06:41:002_0
- RFN: 2705
- Chip: 25856
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 7
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
. (IntegerType)count_I_LSB_UL = -
. (IntegerType)count_I_LSB_DL = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 03 02 01 00

- No.: 1659
- Timestamp: 21:06:41:004_0
- RFN: 2705
- Chip: 32768
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 8
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 1660
- Timestamp: 21:06:41:006_0
- RFN: 2706
- Chip: 1280
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 9
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
. (IntegerType)count_I_LSB_UL = -
. (IntegerType)count_I_LSB_DL = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 04 02 01 00

- No.: 1661
- Timestamp: 21:06:41:008_0
- RFN: 2706
- Chip: 8960
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 10
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 1665
- Timestamp: 21:06:41:011_0
- RFN: 2706
- Chip: 19456
- Event: Send
- PCO: CRLC
- Message: CRLC_Integrity_Activate_REQ
- Source: ts_CRLC_DL_Integrity LINE 1
- Message Structure:
CRLC_Integrity_Activate_REQ
. (IntegerType)cellId = -1
. (CN_DomainIdentity)cn_DomainIdentity = 1
. IntegrityActivationInfo
. . IntegrityProtectionModeInfo
. . . IntegrityProtectionModeCommand
. . . . startIntegrityProtection
. . . . . (BitStringType)integrityProtInitNumber[32] = "00000000000000000000000000000001"
. . . (IntegrityProtectionAlgorithm)integrityProtectionAlgorithm = 0
- Constraint:
ca_CRLC_DL_IntegrityActivateReq
- BinaryMessage:
30 15 02 01 ff 0a 01 01 30 0d 30 30 07 03 05 00 00 00 00 01 0a 01 00

- No.: 1666
- Timestamp: 21:06:41:012_0
- RFN: 2706
- Chip: 25856
- Event: Receive
- PCO: CRLC
- Message: CRLC_Integrity_Activate_CNF
- Source: ts_CRLC_DL_Integrity LINE 2
- Message Structure:
CRLC_Integrity_Activate_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_IntegrityActivateCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1673
- Timestamp: 21:06:41:016_0
- RFN: 2707
- Chip: 2048
- Event: Send
- PCO: CRLC
- Message: CRLC_Integrity_Activate_REQ
- Source: ts_RB2_UL_IntegrityActivate LINE 1
- Message Structure:
CRLC_Integrity_Activate_REQ
. (IntegerType)cellId = -1
. (CN_DomainIdentity)cn_DomainIdentity = 1
. IntegrityActivationInfo
. . IntegrityProtActivationInfoList
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity = 2
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
- Constraint:
ca_CRLC_UL_IntegrityActivateReq
- BinaryMessage:
30 10 02 01 ff 0a 01 01 30 08 30 06 02 01 02 02 01 00

- No.: 1674
- Timestamp: 21:06:41:018_0
- RFN: 2707
- Chip: 8448
- Event: Receive
- PCO: CRLC
- Message: CRLC_Integrity_Activate_CNF
- Source: ts_RB2_UL_IntegrityActivate LINE 2
- Message Structure:
CRLC_Integrity_Activate_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_IntegrityActivateCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1680
- Timestamp: 21:06:41:024_0
- RFN: 2707
- Chip: 32512
- Event: Send
- PCO: AM
- Message: RLC_AM_DATA_REQ
- Source: ts_RRC_Security:lt_SendSecurityModeCommand LINE 7
- Message Structure:
RLC_AM_DATA_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. AmConfirmationRequest
. aM_message
. . DL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00000000000000000000000000000000"
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . DL_DCCH_MessageType
. . . . SecurityModeCommand
. . . . . r3
. . . . . . SecurityModeCommand_r3_IEs
. . . . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . . . SecurityCapability
. . . . . . . . (BitStringType)cipheringAlgorithmCap[16] = '0000000000000011'B
. . . . . . . . (BitStringType)integrityProtectionAlgorithmCap[16] = '0000000000000010'B
. . . . . . . CipheringModeInfo
. . . . . . . IntegrityProtectionModeInfo
. . . . . . . . IntegrityProtectionModeCommand
. . . . . . . . . startIntegrityProtection
. . . . . . . . . . (BitStringType)integrityProtInitNumber[32] = "00000000000000000000000000000001"
. . . . . . . . (IntegrityProtectionAlgorithm)integrityProtectionAlgorithm = 0
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity = 1
. . . . . . . InterRAT_UE_SecurityCapList
. . . . . . laterNonCriticalExtensions
- Constraint:
cas_RRC_SecModeCmd
- BinaryMessage:
30 17 02 01 ff 02 01 02 05 00 80 00 00 00 04 04 00 01 80 01 40 00 00 00 30

- No.: 1686
- Timestamp: 21:06:41:149_0
- RFN: 2720
- Chip: 13312
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_IND
- Source: ts_RRC_Security:lt_StartSecurity_UE LINE 8
- Message Structure:
RLC_AM_DATA_IND
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. IntegrityResult
. . (IntegrityStatus)integrityUsed = 0
. aM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "11101101011010000100111100101101"
. . . . (IntegerType)rrc_MessageSequenceNumber = 1
. . . UL_DCCH_MessageType
. . . . SecurityModeComplete
. . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . IntegrityProtActivationInfo
. . . . . . RRC_MessageSequenceNumberList
. . . . . . . (IntegerType)_elem = 0
. . . . . . . (IntegerType)_elem = 0
. . . . . . . (IntegerType)_elem = 0
. . . . . . . (IntegerType)_elem = 0
. . . . . . . (IntegerType)_elem = 0
. . . . . laterNonCriticalExtensions
. . . . . . (BitStringType)securityModeComplete_r3_add_ext = 0
. . . . . . nonCriticalExtensions
- Constraint:
car_RRC_SecModeCmpl
- BinaryMessage:
30 12 02 01 ff 02 01 02 0a 01 00 f6 b4 27 96 8d 21 00 00 00

- No.: 1687
- Timestamp: 21:06:41:150_0
- RFN: 2720
- Chip: 17408
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_Security:lt_StartSecurity_UE LINE 8
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1689
- Timestamp: 21:06:41:154_0
- RFN: 2720
- Chip: 32512
- Event: Send
- PCO: CRLC
- Message: CRLC_Integrity_Activate_REQ
- Source: ts_CRLC_UL_Integrity LINE 1
- Message Structure:
CRLC_Integrity_Activate_REQ
. (IntegerType)cellId = -1
. (CN_DomainIdentity)cn_DomainIdentity = 1
. IntegrityActivationInfo
. . IntegrityProtActivationInfoList
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity = 0
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity = 1
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity = 3
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity = 4
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
- Constraint:
ca_CRLC_UL_IntegrityActivateReq
- BinaryMessage:
30 28 02 01 ff 0a 01 01 30 20 30 06 02 01 00 02 01 00 30 06 02 01 01 02 01 00 30 06 02 01 03 02 01 00 30 06 02 01 04 02 01 00

- No.: 1690
- Timestamp: 21:06:41:156_0
- RFN: 2721
- Chip: 1280
- Event: Receive
- PCO: CRLC
- Message: CRLC_Integrity_Activate_CNF
- Source: ts_CRLC_UL_Integrity LINE 2
- Message Structure:
CRLC_Integrity_Activate_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_IntegrityActivateCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1702
- Timestamp: 21:06:41:161_0
- RFN: 2721
- Chip: 23040
- Event: Send
- PCO: Dc
- Message: RRC_DataReq
- Source: ts_TC_ActivateRB_TestMode LINE 7
- Message Structure:
RRC_DataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[-1] = -
. (SapId)sapId[1] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. ACTIVATERBTESTMODE
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)tCProtocolDiscriminator[4] = '1111'B
. . (MsgType)msgType[8] = '01000100'B
- Constraint:
ca_PS_DataReq
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 0f 44

- No.: 1703
- Timestamp: 21:06:41:162_0
- RFN: 2721
- Chip: 26624
- Event: Start Timer
- Source: ts_TC_ActivateRB_TestMode LINE 7
- Message Structure:
no details available
- Constraint:
t_Dly (5000 Ms)
- BinaryMessage:

- No.: 1707
- Timestamp: 21:06:41:287_0
- RFN: 2734
- Chip: 5120
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_TC_ActivateRB_TestMode LINE 8
- Message Structure:
RRC_DataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. (START_Value)start[0] = -
. ACTIVATERBTESTMODECOMPLETE
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)tCProtocolDiscriminator[4] = '1111'B
. . (MsgType)msgType[8] = '01000101'B
- Constraint:
car_PS_UplinkDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 0f 45

- No.: 1708
- Timestamp: 21:06:41:288_0
- RFN: 2734
- Chip: 8448
- Event: Cancel Timer
- Source: ts_TC_ActivateRB_TestMode LINE 8
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 1709
- Timestamp: 21:06:41:288_1
- RFN: 2734
- Chip: 9216
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_TC_ActivateRB_TestMode LINE 8
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1728
- Timestamp: 21:06:41:314_0
- RFN: 2736
- Chip: 32256
- Event: Send
- PCO: CPHY
- Message: CPHY_Frame_Number_REQ
- Source: ts_RRC_SetUpRAB_AM_7_RLC LINE 2
- Message Structure:
CPHY_Frame_Number_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
cas_GetFrameNum
- BinaryMessage:
30 06 02 01 00 02 01 1a

- No.: 1732
- Timestamp: 21:06:41:326_0
- RFN: 2738
- Chip: 0
- Event: Receive
- PCO: CPHY
- Message: CPHY_Frame_Number_CNF
- Source: ts_RRC_SetUpRAB_AM_7_RLC LINE 3
- Message Structure:
CPHY_Frame_Number_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
. (IntegerType)frameNumber = 177
- Constraint:
car_GetFrameNum
- BinaryMessage:
30 0a 02 01 00 02 01 1a 02 02 00 b1

- No.: 1736
- Timestamp: 21:06:41:370_0
- RFN: 2742
- Chip: 17152
- Event: Send
- PCO: AM
- Message: RLC_AM_DATA_REQ
- Source: ts_RRC_SetUpRAB_AM_7_RLC:lt_SendRAB_SetupCS_OrPS LINE 4
- Message Structure:
RLC_AM_DATA_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. AmConfirmationRequest
. . (IntegerType)confirmationRequested = 0
. aM_message
. . DL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00000000000000000000000000000000"
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . DL_DCCH_MessageType
. . . . RadioBearerSetup
. . . . . r3
. . . . . . RadioBearerSetup_r3_IEs
. . . . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . . . IntegrityProtectionModeInfo
. . . . . . . CipheringModeInfo
. . . . . . . (IntegerType)activationTime = 168
. . . . . . . U_RNTI
. . . . . . . (BitStringType)new_C_RNTI[16] = -
. . . . . . . (RRC_StateIndicator)rrc_StateIndicator = 0
. . . . . . . (IntegerType)utran_DRX_CycleLengthCoeff = -
. . . . . . . (BitStringType)ura_Identity[0] = -
. . . . . . . CN_InformationInfo
. . . . . . . SRB_InformationSetupList
. . . . . . . RAB_InformationSetupList
. . . . . . . . RAB_InformationSetup
. . . . . . . . . RAB_Info
. . . . . . . . . . RAB_Identity
. . . . . . . . . . . (BitStringType)gsm_MAP_RAB_Identity[8] = '00000101'B
. . . . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = 1
. . . . . . . . . . (BitStringType)nas_Synchronisation_Indicator[0] = -
. . . . . . . . . . (Re_EstablishmentTimer)re_EstablishmentTimer = 0
. . . . . . . . . RB_InformationSetupList
. . . . . . . . . . RB_InformationSetup
. . . . . . . . . . . (IntegerType)rb_Identity = 20
. . . . . . . . . . . PDCP_Info
. . . . . . . . . . . RLC_InfoChoice
. . . . . . . . . . . . RLC_Info
. . . . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . . . MaxDAT_Retransmissions
. . . . . . . . . . . . . . . . . (MaxDAT)maxDAT = 3
. . . . . . . . . . . . . . . . . (TimerMRW)timerMRW = 13
. . . . . . . . . . . . . . . . . (MaxMRW)maxMRW = 1
. . . . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize = 5
. . . . . . . . . . . . . . . (TimerRST)timerRST = 9
. . . . . . . . . . . . . . . (MaxRST)max_RST = 1
. . . . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit = -
. . . . . . . . . . . . . . . . (TimerPoll)timerPoll = -
. . . . . . . . . . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . . . . . . . . . (Poll_SDU)poll_SDU = -
. . . . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . . . (PollWindow)pollWindow = -
. . . . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize = 5
. . . . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit = -
. . . . . . . . . . . . . . . . (TimerEPC)timerEPC = -
. . . . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = 3
. . . . . . . . . . . RB_MappingInfo
. . . . . . . . . . . . RB_MappingOption
. . . . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . . . (IntegerType)dch = 1
. . . . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 7
. . . . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 7
. . . . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . . . (IntegerType)dch = 6
. . . . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 7
. . . . . . . RB_InformationAffectedList
. . . . . . . DL_CounterSynchronisationInfo
. . . . . . . UL_CommonTransChInfo
. . . . . . . . TFC_Subset
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . TFCS
. . . . . . . . . . . ExplicitTFCS_Configuration
. . . . . . . . . . . . TFCS_ReconfAdd
. . . . . . . . . . . . . ctfcSize
. . . . . . . . . . . . . . ctfc4Bit
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . . . . . . . (IntegerType)ctfc4 = 0
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . . . . . . . (IntegerType)ctfc4 = 1
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . . . . . . . (IntegerType)ctfc4 = 2
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . . . . . . . (IntegerType)ctfc4 = 3
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 11
. . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . UL_DeletedTransChInfoList
. . . . . . . UL_AddReconfTransChInfoList
. . . . . . . . UL_AddReconfTransChInformation
. . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType = 0
. . . . . . . . . (IntegerType)transportChannelIdentity = 1
. . . . . . . . . TransportFormatSet
. . . . . . . . . . DedicatedTransChTFS
. . . . . . . . . . . tti
. . . . . . . . . . . . DedicatedDynamicTF_InfoList
. . . . . . . . . . . . . DedicatedDynamicTF_Info
. . . . . . . . . . . . . . rlc_Size
. . . . . . . . . . . . . . . OctetModeRLC_SizeInfoType1
. . . . . . . . . . . . . . . . (IntegerType)sizeType1 = 16
. . . . . . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . LogicalChannelList
. . . . . . . . . . . SemistaticTF_Information
. . . . . . . . . . . . ChannelCodingType
. . . . . . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . . . . . (IntegerType)rateMatchingAttribute = 155
. . . . . . . . . . . . (CRC_Size)crc_Size = 3
. . . . . . . . UL_AddReconfTransChInformation
. . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType = 0
. . . . . . . . . (IntegerType)transportChannelIdentity = 5
. . . . . . . . . TransportFormatSet
. . . . . . . . . . DedicatedTransChTFS
. . . . . . . . . . . tti
. . . . . . . . . . . . DedicatedDynamicTF_InfoList
. . . . . . . . . . . . . DedicatedDynamicTF_Info
. . . . . . . . . . . . . . rlc_Size
. . . . . . . . . . . . . . . BitModeRLC_SizeInfo
. . . . . . . . . . . . . . . . sizeType2
. . . . . . . . . . . . . . . . . (IntegerType)part1 = 2
. . . . . . . . . . . . . . . . . (IntegerType)part2 = -
. . . . . . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . LogicalChannelList
. . . . . . . . . . . SemistaticTF_Information
. . . . . . . . . . . . ChannelCodingType
. . . . . . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . . . . . (IntegerType)rateMatchingAttribute = 170
. . . . . . . . . . . . (CRC_Size)crc_Size = 3
. . . . . . . modeSpecificTransChInfo
. . . . . . . . fdd
. . . . . . . . . (IntegerType)cpch_SetID = -
. . . . . . . . . DRAC_StaticInformationList
. . . . . . . DL_CommonTransChInfo
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . dl_Parameters
. . . . . . . DL_DeletedTransChInfoList
. . . . . . . DL_AddReconfTransChInfoList
. . . . . . . . DL_AddReconfTransChInformation
. . . . . . . . . (DL_TrCH_Type)dl_TransportChannelType = 0
. . . . . . . . . (IntegerType)dl_transportChannelIdentity = 6
. . . . . . . . . tfs_SignallingMode
. . . . . . . . . . UL_TransportChannelIdentity
. . . . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType = 0
. . . . . . . . . . . (IntegerType)ul_TransportChannelIdentity = 1
. . . . . . . . . QualityTarget
. . . . . . . . . . (IntegerType)bler_QualityValue = -20
. . . . . . . . . TM_SignallingInfo
. . . . . . . . DL_AddReconfTransChInformation
. . . . . . . . . (DL_TrCH_Type)dl_TransportChannelType = 0
. . . . . . . . . (IntegerType)dl_transportChannelIdentity = 10
. . . . . . . . . tfs_SignallingMode
. . . . . . . . . . UL_TransportChannelIdentity
. . . . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType = 0
. . . . . . . . . . . (IntegerType)ul_TransportChannelIdentity = 5
. . . . . . . . . QualityTarget
. . . . . . . . . . (IntegerType)bler_QualityValue = -20
. . . . . . . . . TM_SignallingInfo
. . . . . . . FrequencyInfo
. . . . . . . (IntegerType)maxAllowedUL_TX_Power = 33
. . . . . . . UL_ChannelRequirement
. . . . . . . . UL_DPCH_Info
. . . . . . . . . UL_DPCH_PowerControlInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (IntegerType)dpcch_PowerOffset = -40
. . . . . . . . . . . (IntegerType)pc_Preamble = 1
. . . . . . . . . . . (IntegerType)sRB_delay = 7
. . . . . . . . . . . PowerControlAlgorithm
. . . . . . . . . . . . (IntegerType)algorithm1 = 1
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (ScramblingCodeType)scramblingCodeType = 1
. . . . . . . . . . . (IntegerType)scramblingCode = 0
. . . . . . . . . . . (IntegerType)numberOfDPDCH = -
. . . . . . . . . . . (SpreadingFactor)spreadingFactor = 4
. . . . . . . . . . . (BooleanType)tfci_Existence = TRUE
. . . . . . . . . . . (IntegerType)numberOfFBI_Bits = -
. . . . . . . . . . . (PuncturingLimit)puncturingLimit = 15
. . . . . . . modeSpecificPhysChInfo
. . . . . . . . fdd
. . . . . . . . . DL_PDSCH_Information
. . . . . . . DL_CommonInformation
. . . . . . . . DL_DPCH_InfoCommon
. . . . . . . . . cfnHandling
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . DL_DPCH_PowerControlInfo
. . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . (DPC_Mode)dpc_Mode = 0
. . . . . . . . . . . (IntegerType)powerOffsetPilot_pdpdch = 0
. . . . . . . . . . . Dl_rate_matching_restriction
. . . . . . . . . . . SF512_AndPilot
. . . . . . . . . . . . (PilotBits128)sfd128 = 0
. . . . . . . . . . . (PositionFixedOrFlexible)positionFixedOrFlexible = 1
. . . . . . . . . . . (BooleanType)tfci_Existence = TRUE
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . (IntegerType)defaultDPCH_OffsetValue = -
. . . . . . . . . . DPCH_CompressedModeInfo
. . . . . . . . . . (TX_DiversityMode)tx_DiversityMode = 0
. . . . . . . . . . SSDT_Information
. . . . . . . DL_InformationPerRL_List
. . . . . . . . DL_InformationPerRL
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . PrimaryCPICH_Info
. . . . . . . . . . . . (IntegerType)primaryScramblingCode = 100
. . . . . . . . . . . PDSCH_SHO_DCH_Info
. . . . . . . . . . . PDSCH_CodeMapping
. . . . . . . . . DL_DPCH_InfoPerRL
. . . . . . . . . . fdd
. . . . . . . . . . . (PCPICH_UsageForChannelEst)pCPICH_UsageForChannelEst = 0
. . . . . . . . . . . (IntegerType)dpch_FrameOffset = 0
. . . . . . . . . . . SecondaryCPICH_Info
. . . . . . . . . . . DL_ChannelisationCodeList
. . . . . . . . . . . . DL_ChannelisationCode
. . . . . . . . . . . . . (IntegerType)secondaryScramblingCode = 1
. . . . . . . . . . . . . SF512_AndCodeNumber
. . . . . . . . . . . . . . (IntegerType)sf128 = 0
. . . . . . . . . . . . . (ScramblingCodeChange)scramblingCodeChange = -
. . . . . . . . . . . (IntegerType)tpc_CombinationIndex = 0
. . . . . . . . . . . (SSDT_CellIdentity)ssdt_CellIdentity = -
. . . . . . . . . . . (ClosedLoopTimingAdjMode)closedLoopTimingAdjMode = -
. . . . . . . . . SCCPCH_InfoForFACH
. . . . . . v3a0NonCriticalExtensions
. . . . . . . RadioBearerSetup_v3a0ext
. . . . . . . . (BitStringType)new_DSCH_RNTI[16] = -
. . . . . . . laterNonCriticalExtensions
- Constraint:
cas_RB_SetUpAM_WithCnf
- BinaryMessage:
30 4f 02 01 ff 02 01 02 02 01 00 80 00 00 00 03 92 04 ba f2 a0 00 16 09 b3 1e 95 92 06 54 d8 d0 0c e4 2b 10 20 1c 12 29 24 99 5f 81 00 41 20 11 1c d3 10 80 44 11 1d 4b 06 18 58 15 c4 c4 ae 9a 54 7a 20 00 00 13 e4 80 56 20 40 c8 00 01 05 00 00

- No.: 1741
- Timestamp: 21:06:41:528_0
- RFN: 2758
- Chip: 6400
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_CNF
- Source: ts_RRC_SetUpRAB_AM_7_RLC LINE 6
- Message Structure:
RLC_AM_DATA_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. (IntegerType)mui = 0
- Constraint:
car_AM_DataMuiCnf
- BinaryMessage:
30 09 02 01 ff 02 01 02 02 01 00

- No.: 1748
- Timestamp: 21:06:41:655_0
- RFN: 2770
- Chip: 34816
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Modify_REQ
- Source: ts_SS_2DCH_Modify LINE 3
- Message Structure:
CPHY_RL_Modify_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
. (RatType)ratType = 0
. CphyRlModifyReq
. . SS_ActivationTime
. . . (IntegerType)activationCFN = 168
. . physicalChannelInfo
. . . DPCHInfo
. . . . UL_DPCH_Info
. . . . DL_DPCHInfo
. . . . . DL_CommonInformation
. . . . . . DL_DPCH_InfoCommon
. . . . . . . cfnHandling
. . . . . . . modeSpecificInfo
. . . . . . . . fdd
. . . . . . . . . DL_DPCH_PowerControlInfo
. . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . fdd
. . . . . . . . . . . . (DPC_Mode)dpc_Mode = 0
. . . . . . . . . (IntegerType)powerOffsetPilot_pdpdch = 0
. . . . . . . . . Dl_rate_matching_restriction
. . . . . . . . . SF512_AndPilot
. . . . . . . . . . (PilotBits128)sfd128 = 0
. . . . . . . . . (PositionFixedOrFlexible)positionFixedOrFlexible = 1
. . . . . . . . . (BooleanType)tfci_Existence = TRUE
. . . . . . modeSpecificInfo
. . . . . . . fdd
. . . . . . . . (IntegerType)defaultDPCH_OffsetValue = -
. . . . . . . . DPCH_CompressedModeInfo
. . . . . . . . (TX_DiversityMode)tx_DiversityMode = 0
. . . . . . . . SSDT_Information
. . . . . DL_DPCH_InfoPerRL
. . . . . . fdd
. . . . . . . (PCPICH_UsageForChannelEst)pCPICH_UsageForChannelEst = 0
. . . . . . . (IntegerType)dpch_FrameOffset = 0
. . . . . . . SecondaryCPICH_Info
. . . . . . . DL_ChannelisationCodeList
. . . . . . . . DL_ChannelisationCode
. . . . . . . . . (IntegerType)secondaryScramblingCode = 1
. . . . . . . . . SF512_AndCodeNumber
. . . . . . . . . . (IntegerType)sf128 = 0
. . . . . . . . . (ScramblingCodeChange)scramblingCodeChange = -
. . . . . . . (IntegerType)tpc_CombinationIndex = 0
. . . . . . . (SSDT_CellIdentity)ssdt_CellIdentity = -
. . . . . . . (ClosedLoopTimingAdjMode)closedLoopTimingAdjMode = -
. . . . . (IntegerType)powerOffsetOfTFCI_PO1 = 0
. . . . . (IntegerType)powerOffsetOfTPC_PO2 = 0
. . . . . (IntegerType)powerOffsetOfPILOT_PO3 = 0
. . . . . (IntegerType)dl_TxPower = -5
. . . . . (IntegerType)dl_TxPowerMax = 15
. . . . . (IntegerType)dl_TxPowerMin = -35
- Constraint:
ca_DL_DPCH_ModifyInfo
- BinaryMessage:
30 5e 02 01 00 02 01 1a 0a 01 00 30 53 02 02 00 a8 30 4d 30 4b 30 21 30 19 05 00 30 30 14 30 06 30 30 03 0a 01 00 02 01 00 0a 01 00 0a 01 01 01 01 ff 30 30 03 0a 01 00 30 30 13 0a 01 00 02 01 00 30 08 30 06 02 01 01 02 01 00 02 01 00 02 01 00 02 01 00 02 01 00 02 01 fb 02 01 0f 02 01 dd

- No.: 1752
- Timestamp: 21:06:41:704_0
- RFN: 2775
- Chip: 33792
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Modify_CNF
- Source: ts_SS_2DCH_Modify LINE 4
- Message Structure:
CPHY_RL_Modify_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
ca_RL_ModifyCnf
- BinaryMessage:
30 06 02 01 00 02 01 1a

- No.: 1753
- Timestamp: 21:06:41:732_0
- RFN: 2778
- Chip: 24320
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Config_REQ
- Source: ts_SS_2DCH_Modify LINE 5
- Message Structure:
CPHY_TrCH_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
. (RatType)ratType = 0
. CphyTrchConfigReq
. . SS_ActivationTime
. . . (IntegerType)activationCFN = 168
. . ulconnectedTrCHList
. . TFCS
. . dlconnectedTrCHList
. . . CphyTrchConfigReq_setseq_1
. . . . (IntegerType)trchid = 6
. . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 144
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional = 1
. . . . . . (IntegerType)rateMatchingAttribute = 155
. . . . . . (CRC_Size)crc_Size = 3
. . . CphyTrchConfigReq_setseq_1
. . . . (IntegerType)trchid = 10
. . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 148
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional = 1
. . . . . . (IntegerType)rateMatchingAttribute = 170
. . . . . . (CRC_Size)crc_Size = 3
. . TFCS
. . . ExplicitTFCS_Configuration
. . . . TFCS_ReconfAdd
. . . . . ctfcSize
. . . . . . ctfc4Bit
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 0
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 1
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 2
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 3
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . fdd
. . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 9
. . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
- Constraint:
ca_TrChCfgInfo
- BinaryMessage:
30 81 96 02 01 00 02 01 1a 0a 01 00 30 81 8a 02 02 00 a8 30 4c 30 24 02 01 06 0a 01 00 30 1c 30 0e 30 0c 02 02 00 90 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 9b 0a 01 03 30 24 02 01 0a 0a 01 00 30 1c 30 0e 30 0c 02 02 00 94 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 aa 0a 01 03 30 36 30 30 33 30 08 02 01 00 30 03 02 01 00 30 08 02 01 01 30 03 02 01 00 30 08 02 01 02 30 03 02 01 00 30 13 02 01 03 30 0e 30 0c 30 30 03 02 01 09 02 01 0f 02 01 00

- No.: 1757
- Timestamp: 21:06:41:781_0
- RFN: 2783
- Chip: 20992
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Config_CNF
- Source: ts_SS_2DCH_Modify LINE 6
- Message Structure:
CPHY_TrCH_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
ca_TrChCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 1a

- No.: 1758
- Timestamp: 21:06:41:841_0
- RFN: 2789
- Chip: 17152
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_SS_2DCH_Modify LINE 7
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
. (RatType)ratType = 0
. configMessage
. . CmacConfigReq
. . . SS_ActivationTime
. . . . (IntegerType)activationCFN = 168
. . . UE_Info
. . . . U_RNTI
. . . . (BitStringType)c_RNTI[16] = -
. . . TrCHInfo
. . . . ulconnectedTrCHList
. . . . TFCS
. . . . dlconnectedTrCHList
. . . . . TrCHInfo_setseq_1
. . . . . . (IntegerType)trchid = 6
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 144
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . (IntegerType)rateMatchingAttribute = 155
. . . . . . . . (CRC_Size)crc_Size = 3
. . . . . TrCHInfo_setseq_1
. . . . . . (IntegerType)trchid = 10
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 148
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . (IntegerType)rateMatchingAttribute = 170
. . . . . . . . (CRC_Size)crc_Size = 3
. . . . TFCS
. . . . . ExplicitTFCS_Configuration
. . . . . . TFCS_ReconfAdd
. . . . . . . ctfcSize
. . . . . . . . ctfc4Bit
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 0
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 1
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 2
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 3
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 9
. . . . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . TrCH_LogCHMappingList1
. . . . ulconnectedTrCHList
. . . . dlconnectedTrCHList
. . . . . TrCH_LogCHMappingList1_setseq_1
. . . . . . (IntegerType)trchid = 6
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 7
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 5
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 7
. . . . . . . . (IntegerType)rB_Identity = -12
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . TrCH_LogCHMappingList1_setseq_1
. . . . . . (IntegerType)trchid = 10
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 1
. . . . . . . . (IntegerType)rB_Identity = 1
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 2
. . . . . . . . (IntegerType)rB_Identity = 2
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 3
. . . . . . . . (IntegerType)rB_Identity = 3
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 4
. . . . . . . . (IntegerType)rB_Identity = 4
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_CMAC_ReconfigInfo
- BinaryMessage:
30 82 01 22 02 01 ff 02 01 1a 0a 01 00 30 82 01 15 02 02 00 a8 30 00 30 81 80 30 46 30 21 02 01 06 30 1c 30 0e 30 0c 02 02 00 90 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 9b 0a 01 03 30 21 02 01 0a 30 1c 30 0e 30 0c 02 02 00 94 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 aa 0a 01 03 30 36 30 30 33 30 08 02 01 00 30 03 02 01 00 30 08 02 01 01 30 03 02 01 00 30 08 02 01 02 30 03 02 01 00 30 13 02 01 03 30 0e 30 0c 30 30 03 02 01 09 02 01 0f 02 01 00 30 81 89 30 81 86 30 1d 02 01 06 30 18 30 16 30 11 0a 01 00 0a 01 00 02 01 07 0a 01 05 05 00 02 01 07 02 01 f4 30 65 02 01 0a 30 60 30 16 30 11 0a 01 00 0a 01 00 02 01 01 0a 01 04 05 00 02 01 01 02 01 01 30 16 30 11 0a 01 00 0a 01 00 02 01 02 0a 01 04 05 00 02 01 02 02 01 02 30 16 30 11 0a 01 00 0a 01 00 02 01 03 0a 01 04 05 00 02 01 03 02 01 03 30 16 30 11 0a 01 00 0a 01 00 02 01 04 0a 01 04 05 00 02 01 04 02 01 04

- No.: 1759
- Timestamp: 21:06:41:875_0
- RFN: 2792
- Chip: 35072
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_SS_2DCH_Modify LINE 8
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 1a

- No.: 1760
- Timestamp: 21:06:41:902_0
- RFN: 2795
- Chip: 24320
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Modify_REQ
- Source: ts_SS_2DCH_Modify LINE 9
- Message Structure:
CPHY_RL_Modify_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
. (RatType)ratType = 0
. CphyRlModifyReq
. . SS_ActivationTime
. . . (IntegerType)activationCFN = 168
. . physicalChannelInfo
. . . DPCHInfo
. . . . UL_DPCH_Info
. . . . . UL_DPCH_PowerControlInfo
. . . . . . fdd
. . . . . . . (IntegerType)dpcch_PowerOffset = -40
. . . . . . . (IntegerType)pc_Preamble = 1
. . . . . . . (IntegerType)sRB_delay = 7
. . . . . . . PowerControlAlgorithm
. . . . . . . . (IntegerType)algorithm1 = 1
. . . . . modeSpecificInfo
. . . . . . fdd
. . . . . . . (ScramblingCodeType)scramblingCodeType = 1
. . . . . . . (IntegerType)scramblingCode = 0
. . . . . . . (IntegerType)numberOfDPDCH = -
. . . . . . . (SpreadingFactor)spreadingFactor = 4
. . . . . . . (BooleanType)tfci_Existence = TRUE
. . . . . . . (IntegerType)numberOfFBI_Bits = -
. . . . . . . (PuncturingLimit)puncturingLimit = 15
. . . . DL_DPCHInfo
- Constraint:
ca_UL_DPCH_ModifyInfo
- BinaryMessage:
30 34 02 01 00 02 01 14 0a 01 00 30 29 02 02 00 a8 30 23 30 21 30 30 0c 02 01 d8 02 01 01 02 01 07 02 01 01 30 30 0f 0a 01 01 02 01 00 0a 01 04 01 01 ff 0a 01 0f

- No.: 1764
- Timestamp: 21:06:41:953_0
- RFN: 2800
- Chip: 26624
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Modify_CNF
- Source: ts_SS_2DCH_Modify LINE 10
- Message Structure:
CPHY_RL_Modify_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_RL_ModifyCnf
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 1765
- Timestamp: 21:06:41:981_0
- RFN: 2803
- Chip: 22016
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Config_REQ
- Source: ts_SS_2DCH_Modify LINE 11
- Message Structure:
CPHY_TrCH_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
. (RatType)ratType = 0
. CphyTrchConfigReq
. . SS_ActivationTime
. . . (IntegerType)activationCFN = 168
. . ulconnectedTrCHList
. . . CphyTrchConfigReq_setseq_0
. . . . (IntegerType)trchid = 1
. . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 144
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional = 1
. . . . . . (IntegerType)rateMatchingAttribute = 155
. . . . . . (CRC_Size)crc_Size = 3
. . . CphyTrchConfigReq_setseq_0
. . . . (IntegerType)trchid = 5
. . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 148
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional = 1
. . . . . . (IntegerType)rateMatchingAttribute = 170
. . . . . . (CRC_Size)crc_Size = 3
. . TFCS
. . . ExplicitTFCS_Configuration
. . . . TFCS_ReconfAdd
. . . . . ctfcSize
. . . . . . ctfc4Bit
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 0
. . . . . . . . PowerOffsetInformation
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 1
. . . . . . . . PowerOffsetInformation
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 2
. . . . . . . . PowerOffsetInformation
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 3
. . . . . . . . PowerOffsetInformation
. . dlconnectedTrCHList
. . TFCS
- Constraint:
ca_TrChCfgInfo
- BinaryMessage:
30 76 02 01 00 02 01 14 0a 01 00 30 6b 02 02 00 a8 30 4c 30 24 02 01 01 0a 01 00 30 1c 30 0e 30 0c 02 02 00 90 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 9b 0a 01 03 30 24 02 01 05 0a 01 00 30 1c 30 0e 30 0c 02 02 00 94 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 aa 0a 01 03 30 17 30 30 14 30 03 02 01 00 30 03 02 01 01 30 03 02 01 02 30 03 02 01 03

- No.: 1769
- Timestamp: 21:06:42:032_0
- RFN: 2808
- Chip: 24832
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Config_CNF
- Source: ts_SS_2DCH_Modify LINE 12
- Message Structure:
CPHY_TrCH_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_TrChCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 1770
- Timestamp: 21:06:42:095_0
- RFN: 2814
- Chip: 38144
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_SS_2DCH_Modify LINE 13
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
. (RatType)ratType = 0
. configMessage
. . CmacConfigReq
. . . SS_ActivationTime
. . . . (IntegerType)activationCFN = 168
. . . UE_Info
. . . . U_RNTI
. . . . (BitStringType)c_RNTI[16] = -
. . . TrCHInfo
. . . . ulconnectedTrCHList
. . . . . TrCHInfo_setseq_0
. . . . . . (IntegerType)trchid = 1
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 144
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . (IntegerType)rateMatchingAttribute = 155
. . . . . . . . (CRC_Size)crc_Size = 3
. . . . . TrCHInfo_setseq_0
. . . . . . (IntegerType)trchid = 5
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 148
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . (IntegerType)rateMatchingAttribute = 170
. . . . . . . . (CRC_Size)crc_Size = 3
. . . . TFCS
. . . . . ExplicitTFCS_Configuration
. . . . . . TFCS_ReconfAdd
. . . . . . . ctfcSize
. . . . . . . . ctfc4Bit
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 0
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 1
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 2
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 3
. . . . . . . . . . PowerOffsetInformation
. . . . dlconnectedTrCHList
. . . . TFCS
. . . TrCH_LogCHMappingList1
. . . . ulconnectedTrCHList
. . . . . TrCH_LogCHMappingList1_setseq_0
. . . . . . (IntegerType)trchid = 1
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 7
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 5
. . . . . . . . (IntegerType)rB_Identity = -12
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . TrCH_LogCHMappingList1_setseq_0
. . . . . . (IntegerType)trchid = 5
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . (IntegerType)rB_Identity = 1
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . (IntegerType)rB_Identity = 2
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . (IntegerType)rB_Identity = 3
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . (IntegerType)rB_Identity = 4
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . dlconnectedTrCHList
- Constraint:
ca_CMAC_ReconfigInfo
- BinaryMessage:
30 81 e6 02 01 ff 02 01 14 0a 01 00 30 81 da 02 02 00 a8 30 00 30 61 30 46 30 21 02 01 01 30 1c 30 0e 30 0c 02 02 00 90 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 9b 0a 01 03 30 21 02 01 05 30 1c 30 0e 30 0c 02 02 00 94 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 aa 0a 01 03 30 17 30 30 14 30 03 02 01 00 30 03 02 01 01 30 03 02 01 02 30 03 02 01 03 30 6f 30 6d 30 18 02 01 01 30 13 30 11 30 0c 0a 01 00 0a 01 00 02 01 07 0a 01 05 02 01 f4 30 51 02 01 05 30 4c 30 11 30 0c 0a 01 00 0a 01 00 02 01 01 0a 01 04 02 01 01 30 11 30 0c 0a 01 00 0a 01 00 02 01 02 0a 01 04 02 01 02 30 11 30 0c 0a 01 00 0a 01 00 02 01 03 0a 01 04 02 01 03 30 11 30 0c 0a 01 00 0a 01 00 02 01 04 0a 01 04 02 01 04

- No.: 1771
- Timestamp: 21:06:42:129_0
- RFN: 2818
- Chip: 9472
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_SS_2DCH_Modify LINE 14
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 14

- No.: 1774
- Timestamp: 21:06:42:140_0
- RFN: 2819
- Chip: 14080
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB_TM_Cfg_RLC LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = -12
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_TM_RLC_Mode
. . . . . . (BooleanType)segmentationIndication = TRUE
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 144
. . . . . UL_RLC_Mode
. . . . . . UL_TM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . (BooleanType)segmentationIndication = TRUE
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = 7
. . . . (IntegerType)dLlogicalChannelIdentity = 7
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_TM_Info
- BinaryMessage:
30 25 02 01 ff 02 01 f4 0a 01 00 30 1a 30 10 30 03 01 01 ff 30 09 02 02 00 90 30 03 01 01 ff 30 06 02 01 07 02 01 07

- No.: 1778
- Timestamp: 21:06:42:151_0
- RFN: 2820
- Chip: 18944
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB_TM_Cfg_RLC LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = -12
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 f4

- No.: 1786
- Timestamp: 21:06:42:160_1
- RFN: 2821
- Chip: 14848
- Event: Start Timer
- Source: ts_RRC_ReceiveRB_SetupCmpl LINE 2
- Message Structure:
no details available
- Constraint:
t_WaitMS (13500 Ms)
- BinaryMessage:

- No.: 1795
- Timestamp: 21:06:43:894_0
- RFN: 2994
- Chip: 34304
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_IND
- Source: ts_RRC_ReceiveRB_SetupCmpl:lt_CipheringNotStartedAM_RAB LINE 4
- Message Structure:
RLC_AM_DATA_IND
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. IntegrityResult
. . (IntegrityStatus)integrityUsed = 0
. aM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "01100111110100110110111001101110"
. . . . (IntegerType)rrc_MessageSequenceNumber = 2
. . . UL_DCCH_MessageType
. . . . RadioBearerSetupComplete
. . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . IntegrityProtActivationInfo
. . . . . (IntegerType)ul_TimingAdvance = 0
. . . . . (BitStringType)start_Value[20] = "00000000000000000100"
. . . . . (IntegerType)count_C_ActivationTime = 0
. . . . . UL_CounterSynchronisationInfo
. . . . . laterNonCriticalExtensions
. . . . . . (BitStringType)radioBearerSetupComplete_r3_add_ext = 0
. . . . . . nonCriticalExtensions
- Constraint:
car_RB_SetUpCmpl
- BinaryMessage:
30 12 02 01 ff 02 01 02 0a 01 00 b3 e9 b7 37 13 c8 00 00 08

- No.: 1796
- Timestamp: 21:06:43:896_0
- RFN: 2995
- Chip: 1280
- Event: Cancel Timer
- Source: ts_RRC_ReceiveRB_SetupCmpl:lt_CipheringNotStartedAM_RAB LINE 4
- Message Structure:
no details available
- Constraint:
t_WaitMS
- BinaryMessage:

- No.: 1797
- Timestamp: 21:06:43:896_1
- RFN: 2995
- Chip: 2048
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ReceiveRB_SetupCmpl:lt_CipheringNotStartedAM_RAB LINE 4
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1825
- Timestamp: 21:06:43:936_0
- RFN: 2999
- Chip: 1792
- Event: Start Timer
- Source: tc_7_2_3_26:lt_TimerStatusPeriodicTest LINE 4
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 1827
- Timestamp: 21:06:43:939_1
- RFN: 2999
- Chip: 14080
- Event: Start Timer
- Source: tc_7_2_3_26:lt_TimerStatusPeriodicTest LINE 5
- Message Structure:
no details available
- Constraint:
t_Status (10000 Ms)
- BinaryMessage:

- No.: 1835
- Timestamp: 21:06:43:959_1
- RFN: 3001
- Chip: 13312
- Event: Timeout
- Source: tc_7_2_3_26:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 1855
- Timestamp: 21:06:44:003_0
- RFN: 3005
- Chip: 24064
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000000'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'FFE665A5C5CA3452085408ABEECE4B'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 01 1e ff e6 65 a5 c5 ca 34 52 08 54 08 ab ee ce 4b

- No.: 1864
- Timestamp: 21:06:44:016_0
- RFN: 3006
- Chip: 36096
- Event: Start Timer
- Source: tc_7_2_3_26:lt_TxAndRx LINE 16
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 1865
- Timestamp: 21:06:44:016_1
- RFN: 3006
- Chip: 37120
- Event: Repeat
- Source: tc_7_2_3_26:lt_TimerStatusPeriodicTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1870
- Timestamp: 21:06:44:038_0
- RFN: 3009
- Chip: 5888
- Event: Timeout
- Source: tc_7_2_3_26:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 1890
- Timestamp: 21:06:44:076_0
- RFN: 3013
- Chip: 512
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000001'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '0B813FD337873F2CD1E29AE91BD6C8'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 09 1e 0b 81 3f d3 37 87 3f 2c d1 e2 9a e9 1b d6 c8

- No.: 1899
- Timestamp: 21:06:44:089_1
- RFN: 3014
- Chip: 12800
- Event: Start Timer
- Source: tc_7_2_3_26:lt_TxAndRx LINE 16
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 1900
- Timestamp: 21:06:44:090_0
- RFN: 3014
- Chip: 13824
- Event: Repeat
- Source: tc_7_2_3_26:lt_TimerStatusPeriodicTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1905
- Timestamp: 21:06:44:104_0
- RFN: 3015
- Chip: 30208
- Event: Timeout
- Source: tc_7_2_3_26:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 1925
- Timestamp: 21:06:44:143_0
- RFN: 3019
- Chip: 26112
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000010'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'E14FDE630F8195688EBE465F09816A'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 11 1e e1 4f de 63 0f 81 95 68 8e be 46 5f 09 81 6a

- No.: 1934
- Timestamp: 21:06:44:156_0
- RFN: 3021
- Chip: 256
- Event: Start Timer
- Source: tc_7_2_3_26:lt_TxAndRx LINE 16
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 1935
- Timestamp: 21:06:44:156_1
- RFN: 3021
- Chip: 1024
- Event: Repeat
- Source: tc_7_2_3_26:lt_TimerStatusPeriodicTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1940
- Timestamp: 21:06:44:171_1
- RFN: 3022
- Chip: 19456
- Event: Timeout
- Source: tc_7_2_3_26:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 1960
- Timestamp: 21:06:44:209_0
- RFN: 3026
- Chip: 13824
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000011'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '8EEB1B83953DD362DAE3B06D5B76D8'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 19 1e 8e eb 1b 83 95 3d d3 62 da e3 b0 6d 5b 76 d8

- No.: 1969
- Timestamp: 21:06:44:224_0
- RFN: 3027
- Chip: 31488
- Event: Start Timer
- Source: tc_7_2_3_26:lt_TxAndRx LINE 16
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 1970
- Timestamp: 21:06:44:224_1
- RFN: 3027
- Chip: 32256
- Event: Repeat
- Source: tc_7_2_3_26:lt_TimerStatusPeriodicTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1975
- Timestamp: 21:06:44:249_0
- RFN: 3030
- Chip: 12288
- Event: Timeout
- Source: tc_7_2_3_26:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 1995
- Timestamp: 21:06:44:290_0
- RFN: 3034
- Chip: 17408
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000100'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'E3E53087EA645A09017FD99C3CACBB'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 21 1e e3 e5 30 87 ea 64 5a 09 01 7f d9 9c 3c ac bb

- No.: 2004
- Timestamp: 21:06:44:303_0
- RFN: 3035
- Chip: 29440
- Event: Start Timer
- Source: tc_7_2_3_26:lt_TxAndRx LINE 16
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 2005
- Timestamp: 21:06:44:303_1
- RFN: 3035
- Chip: 30464
- Event: Repeat
- Source: tc_7_2_3_26:lt_TimerStatusPeriodicTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2008
- Timestamp: 21:06:44:310_0
- RFN: 3036
- Chip: 12800
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_26:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. STATUS_PDU
. . (DC_Field)dC_Field[1] = '0'B
. . (CtrlPDU_Type)type[3] = '000'B
. . SuperFields
. . (HexStringType)superFieldsAndPadRx[35] = '20020000000000000000000000000000000'H
. . (Padding)paddingTx[0] = -
- Constraint:
car_StatusInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 02 00 20 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00

- No.: 2012
- Timestamp: 21:06:44:318_0
- RFN: 3037
- Chip: 6400
- Event: Start Timer
- Source: tc_7_2_3_26:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_LowerBound (305 Ms)
- BinaryMessage:

- No.: 2013
- Timestamp: 21:06:44:318_1
- RFN: 3037
- Chip: 7680
- Event: Start Timer
- Source: tc_7_2_3_26:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_UpperBound (495 Ms)
- BinaryMessage:

- No.: 2014
- Timestamp: 21:06:44:318_2
- RFN: 3037
- Chip: 9216
- Event: Repeat
- Source: tc_7_2_3_26:lt_TimerStatusPeriodicTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2019
- Timestamp: 21:06:44:325_1
- RFN: 3037
- Chip: 34816
- Event: Timeout
- Source: tc_7_2_3_26:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 2039
- Timestamp: 21:06:44:364_0
- RFN: 3041
- Chip: 30464
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000101'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '46DF1CD61DA9C435F89943DF9CC34A'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 29 1e 46 df 1c d6 1d a9 c4 35 f8 99 43 df 9c c3 4a

- No.: 2048
- Timestamp: 21:06:44:377_1
- RFN: 3043
- Chip: 4608
- Event: Start Timer
- Source: tc_7_2_3_26:lt_TxAndRx LINE 16
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 2049
- Timestamp: 21:06:44:378_0
- RFN: 3043
- Chip: 5632
- Event: Repeat
- Source: tc_7_2_3_26:lt_TimerStatusPeriodicTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2054
- Timestamp: 21:06:44:394_1
- RFN: 3044
- Chip: 30208
- Event: Timeout
- Source: tc_7_2_3_26:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 2074
- Timestamp: 21:06:44:433_0
- RFN: 3048
- Chip: 28416
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000110'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'DEE31AD6E24FA1903D53778D949742'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 31 1e de e3 1a d6 e2 4f a1 90 3d 53 77 8d 94 97 42

- No.: 2083
- Timestamp: 21:06:44:446_1
- RFN: 3050
- Chip: 1792
- Event: Start Timer
- Source: tc_7_2_3_26:lt_TxAndRx LINE 16
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 2084
- Timestamp: 21:06:44:447_0
- RFN: 3050
- Chip: 2816
- Event: Repeat
- Source: tc_7_2_3_26:lt_TimerStatusPeriodicTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2089
- Timestamp: 21:06:44:464_1
- RFN: 3051
- Chip: 30720
- Event: Timeout
- Source: tc_7_2_3_26:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 2109
- Timestamp: 21:06:44:503_0
- RFN: 3055
- Chip: 28160
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000111'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '750DD49DE9CE9E430AD448A14575D8'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 39 1e 75 0d d4 9d e9 ce 9e 43 0a d4 48 a1 45 75 d8

- No.: 2118
- Timestamp: 21:06:44:516_1
- RFN: 3057
- Chip: 1792
- Event: Start Timer
- Source: tc_7_2_3_26:lt_TxAndRx LINE 16
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 2119
- Timestamp: 21:06:44:516_2
- RFN: 3057
- Chip: 2816
- Event: Repeat
- Source: tc_7_2_3_26:lt_TimerStatusPeriodicTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2124
- Timestamp: 21:06:44:534_1
- RFN: 3058
- Chip: 32000
- Event: Timeout
- Source: tc_7_2_3_26:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 2144
- Timestamp: 21:06:44:573_0
- RFN: 3062
- Chip: 30208
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000001000'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '9C160255088140200555DDC9CBCB9E'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 41 1e 9c 16 02 55 08 81 40 20 05 55 dd c9 cb cb 9e

- No.: 2153
- Timestamp: 21:06:44:586_1
- RFN: 3064
- Chip: 3840
- Event: Start Timer
- Source: tc_7_2_3_26:lt_TxAndRx LINE 16
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 2154
- Timestamp: 21:06:44:587_0
- RFN: 3064
- Chip: 4864
- Event: Repeat
- Source: tc_7_2_3_26:lt_TimerStatusPeriodicTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2159
- Timestamp: 21:06:44:604_0
- RFN: 3065
- Chip: 32256
- Event: Timeout
- Source: tc_7_2_3_26:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 2179
- Timestamp: 21:06:44:644_0
- RFN: 3069
- Chip: 28416
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000001001'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'C31F833F866A5BA390680EAB11282E'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 49 1e c3 1f 83 3f 86 6a 5b a3 90 68 0e ab 11 28 2e

- No.: 2188
- Timestamp: 21:06:44:657_1
- RFN: 3071
- Chip: 3072
- Event: Start Timer
- Source: tc_7_2_3_26:lt_TxAndRx LINE 16
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 2189
- Timestamp: 21:06:44:657_2
- RFN: 3071
- Chip: 4096
- Event: Repeat
- Source: tc_7_2_3_26:lt_TimerStatusPeriodicTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2192
- Timestamp: 21:06:44:661_0
- RFN: 3071
- Chip: 17152
- Event: Timeout
- Source: tc_7_2_3_26:lt_TxAndRx LINE 1
- Message Structure:
no details available
- Constraint:
t_LowerBound
- BinaryMessage:

- No.: 2194
- Timestamp: 21:06:44:664_1
- RFN: 3071
- Chip: 32000
- Event: Repeat
- Source: tc_7_2_3_26:lt_TimerStatusPeriodicTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2199
- Timestamp: 21:06:44:675_0
- RFN: 3072
- Chip: 34048
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_26:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. STATUS_PDU
. . (DC_Field)dC_Field[1] = '0'B
. . (CtrlPDU_Type)type[3] = '000'B
. . SuperFields
. . (HexStringType)superFieldsAndPadRx[35] = '20080000000000000000000000000000000'H
. . (Padding)paddingTx[0] = -
- Constraint:
car_StatusInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 02 00 80 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00

- No.: 2203
- Timestamp: 21:06:44:683_1
- RFN: 3073
- Chip: 27904
- Event: Cancel Timer
- Source: tc_7_2_3_26:lt_TxAndRx LINE 9
- Message Structure:
no details available
- Constraint:
t_UpperBound
- BinaryMessage:

- No.: 2204
- Timestamp: 21:06:44:684_0
- RFN: 3073
- Chip: 28672
- Event: Repeat
- Source: tc_7_2_3_26:lt_TimerStatusPeriodicTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2207
- Timestamp: 21:06:44:687_0
- RFN: 3074
- Chip: 2048
- Event: Timeout
- Source: tc_7_2_3_26:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 2227
- Timestamp: 21:06:44:726_0
- RFN: 3078
- Chip: 1280
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000001010'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'AE44F5E7658F6B247A0C54A21057F7'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 51 1e ae 44 f5 e7 65 8f 6b 24 7a 0c 54 a2 10 57 f7

- No.: 2236
- Timestamp: 21:06:44:739_1
- RFN: 3079
- Chip: 13568
- Event: Start Timer
- Source: tc_7_2_3_26:lt_TxAndRx LINE 16
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 2237
- Timestamp: 21:06:44:740_0
- RFN: 3079
- Chip: 14848
- Event: Repeat
- Source: tc_7_2_3_26:lt_TimerStatusPeriodicTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2242
- Timestamp: 21:06:44:755_1
- RFN: 3080
- Chip: 34560
- Event: Timeout
- Source: tc_7_2_3_26:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 2262
- Timestamp: 21:06:44:794_0
- RFN: 3084
- Chip: 33536
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000001011'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '3278595C235077F267A59097E8CEB4'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 59 1e 32 78 59 5c 23 50 77 f2 67 a5 90 97 e8 ce b4

- No.: 2271
- Timestamp: 21:06:44:808_0
- RFN: 3086
- Chip: 7168
- Event: Start Timer
- Source: tc_7_2_3_26:lt_TxAndRx LINE 16
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 2272
- Timestamp: 21:06:44:808_1
- RFN: 3086
- Chip: 8192
- Event: Repeat
- Source: tc_7_2_3_26:lt_TimerStatusPeriodicTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2277
- Timestamp: 21:06:44:825_1
- RFN: 3087
- Chip: 35328
- Event: Timeout
- Source: tc_7_2_3_26:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 2297
- Timestamp: 21:06:44:864_0
- RFN: 3091
- Chip: 32768
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000001100'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'EDE49A16FDB36D2485EA3107D59DC3'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 61 1e ed e4 9a 16 fd b3 6d 24 85 ea 31 07 d5 9d c3

- No.: 2306
- Timestamp: 21:06:44:876_0
- RFN: 3093
- Chip: 768
- Event: Start Timer
- Source: tc_7_2_3_26:lt_TxAndRx LINE 16
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 2307
- Timestamp: 21:06:44:876_1
- RFN: 3093
- Chip: 1536
- Event: Repeat
- Source: tc_7_2_3_26:lt_TimerStatusPeriodicTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2312
- Timestamp: 21:06:44:894_1
- RFN: 3094
- Chip: 34048
- Event: Timeout
- Source: tc_7_2_3_26:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 2332
- Timestamp: 21:06:44:931_0
- RFN: 3098
- Chip: 22784
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000001101'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '60700D5488BEB9B96C24AF44DF498B'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 69 1e 60 70 0d 54 88 be b9 b9 6c 24 af 44 df 49 8b

- No.: 2341
- Timestamp: 21:06:44:945_1
- RFN: 3099
- Chip: 34816
- Event: Start Timer
- Source: tc_7_2_3_26:lt_TxAndRx LINE 16
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 2342
- Timestamp: 21:06:44:946_0
- RFN: 3099
- Chip: 35840
- Event: Repeat
- Source: tc_7_2_3_26:lt_TimerStatusPeriodicTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2347
- Timestamp: 21:06:44:966_1
- RFN: 3101
- Chip: 37632
- Event: Timeout
- Source: tc_7_2_3_26:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 2367
- Timestamp: 21:06:45:005_0
- RFN: 3105
- Chip: 34816
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000001110'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'C135788C14A8BBEC64A5EF64DA1C56'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 71 1e c1 35 78 8c 14 a8 bb ec 64 a5 ef 64 da 1c 56

- No.: 2376
- Timestamp: 21:06:45:018_1
- RFN: 3107
- Chip: 8192
- Event: Start Timer
- Source: tc_7_2_3_26:lt_TxAndRx LINE 16
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 2377
- Timestamp: 21:06:45:018_2
- RFN: 3107
- Chip: 8960
- Event: Repeat
- Source: tc_7_2_3_26:lt_TimerStatusPeriodicTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2382
- Timestamp: 21:06:45:032_1
- RFN: 3108
- Chip: 23040
- Event: Timeout
- Source: tc_7_2_3_26:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 2402
- Timestamp: 21:06:45:073_0
- RFN: 3112
- Chip: 28928
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000001111'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '08FEB312D7B738D3E2CFB4C74A7458'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 79 1e 08 fe b3 12 d7 b7 38 d3 e2 cf b4 c7 4a 74 58

- No.: 2411
- Timestamp: 21:06:45:087_0
- RFN: 3114
- Chip: 3840
- Event: Start Timer
- Source: tc_7_2_3_26:lt_TxAndRx LINE 16
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 2412
- Timestamp: 21:06:45:087_1
- RFN: 3114
- Chip: 4864
- Event: Repeat
- Source: tc_7_2_3_26:lt_TimerStatusPeriodicTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2415
- Timestamp: 21:06:45:093_0
- RFN: 3114
- Chip: 26368
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_26:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. STATUS_PDU
. . (DC_Field)dC_Field[1] = '0'B
. . (CtrlPDU_Type)type[3] = '000'B
. . SuperFields
. . (HexStringType)superFieldsAndPadRx[35] = '200D0000000000000000000000000000000'H
. . (Padding)paddingTx[0] = -
- Constraint:
car_StatusInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 02 00 d0 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00

- No.: 2418
- Timestamp: 21:06:45:098_1
- RFN: 3115
- Chip: 9216
- Event: Repeat
- Source: tc_7_2_3_26:lt_TimerStatusPeriodicTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2423
- Timestamp: 21:06:45:114_0
- RFN: 3116
- Chip: 30208
- Event: Timeout
- Source: tc_7_2_3_26:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 2443
- Timestamp: 21:06:45:153_0
- RFN: 3120
- Chip: 27648
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000010000'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'A3EF9B3C79F3CD348740DFE330780C'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 81 1e a3 ef 9b 3c 79 f3 cd 34 87 40 df e3 30 78 0c

- No.: 2452
- Timestamp: 21:06:45:166_1
- RFN: 3122
- Chip: 2560
- Event: Start Timer
- Source: tc_7_2_3_26:lt_TxAndRx LINE 16
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 2453
- Timestamp: 21:06:45:166_2
- RFN: 3122
- Chip: 3328
- Event: Repeat
- Source: tc_7_2_3_26:lt_TimerStatusPeriodicTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2458
- Timestamp: 21:06:45:186_0
- RFN: 3124
- Chip: 1024
- Event: Timeout
- Source: tc_7_2_3_26:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 2478
- Timestamp: 21:06:45:226_0
- RFN: 3128
- Chip: 1792
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000010001'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '01FFCCCB4B8B9468A410A81157DD9C'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 89 1e 01 ff cc cb 4b 8b 94 68 a4 10 a8 11 57 dd 9c

- No.: 2487
- Timestamp: 21:06:45:240_1
- RFN: 3129
- Chip: 17920
- Event: Start Timer
- Source: tc_7_2_3_26:lt_TxAndRx LINE 16
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 2488
- Timestamp: 21:06:45:240_2
- RFN: 3129
- Chip: 18944
- Event: Repeat
- Source: tc_7_2_3_26:lt_TimerStatusPeriodicTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2493
- Timestamp: 21:06:45:260_0
- RFN: 3131
- Chip: 13056
- Event: Timeout
- Source: tc_7_2_3_26:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 2513
- Timestamp: 21:06:45:299_0
- RFN: 3135
- Chip: 9984
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000010010'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '9617027FA66F0E7E59A3C535D237AD'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 91 1e 96 17 02 7f a6 6f 0e 7e 59 a3 c5 35 d2 37 ad

- No.: 2522
- Timestamp: 21:06:45:312_1
- RFN: 3136
- Chip: 23808
- Event: Start Timer
- Source: tc_7_2_3_26:lt_TxAndRx LINE 16
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 2523
- Timestamp: 21:06:45:313_0
- RFN: 3136
- Chip: 24576
- Event: Repeat
- Source: tc_7_2_3_26:lt_TimerStatusPeriodicTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2528
- Timestamp: 21:06:45:333_0
- RFN: 3138
- Chip: 25856
- Event: Timeout
- Source: tc_7_2_3_26:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 2548
- Timestamp: 21:06:45:372_0
- RFN: 3142
- Chip: 23808
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000010011'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '91C29FBCC61F032AD11D7C8CBE1302'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 99 1e 91 c2 9f bc c6 1f 03 2a d1 1d 7c 8c be 13 02

- No.: 2557
- Timestamp: 21:06:45:386_0
- RFN: 3143
- Chip: 37120
- Event: Start Timer
- Source: tc_7_2_3_26:lt_TxAndRx LINE 16
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 2558
- Timestamp: 21:06:45:386_1
- RFN: 3143
- Chip: 38144
- Event: Repeat
- Source: tc_7_2_3_26:lt_TimerStatusPeriodicTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2563
- Timestamp: 21:06:45:415_1
- RFN: 3146
- Chip: 35072
- Event: Timeout
- Source: tc_7_2_3_26:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 2583
- Timestamp: 21:06:45:455_0
- RFN: 3150
- Chip: 34560
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000010100'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'D51DD637072A7BA6C5B5C760DAB6ED'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 a1 1e d5 1d d6 37 07 2a 7b a6 c5 b5 c7 60 da b6 ed

- No.: 2592
- Timestamp: 21:06:45:471_0
- RFN: 3152
- Chip: 19456
- Event: Start Timer
- Source: tc_7_2_3_26:lt_TxAndRx LINE 16
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 2593
- Timestamp: 21:06:45:471_1
- RFN: 3152
- Chip: 20224
- Event: Repeat
- Source: tc_7_2_3_26:lt_TimerStatusPeriodicTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2596
- Timestamp: 21:06:45:476_0
- RFN: 3153
- Chip: 3072
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_26:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. STATUS_PDU
. . (DC_Field)dC_Field[1] = '0'B
. . (CtrlPDU_Type)type[3] = '000'B
. . SuperFields
. . (HexStringType)superFieldsAndPadRx[35] = '20130000000000000000000000000000000'H
. . (Padding)paddingTx[0] = -
- Constraint:
car_StatusInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 02 01 30 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00

- No.: 2599
- Timestamp: 21:06:45:482_1
- RFN: 3153
- Chip: 24832
- Event: Repeat
- Source: tc_7_2_3_26:lt_TimerStatusPeriodicTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2604
- Timestamp: 21:06:45:487_1
- RFN: 3154
- Chip: 7168
- Event: Timeout
- Source: tc_7_2_3_26:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 2624
- Timestamp: 21:06:45:527_0
- RFN: 3158
- Chip: 6400
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000010101'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'B1C7CA610FD4C8B41202FFB3387959'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 a9 1e b1 c7 ca 61 0f d4 c8 b4 12 02 ff b3 38 79 59

- No.: 2633
- Timestamp: 21:06:45:540_1
- RFN: 3159
- Chip: 19200
- Event: Start Timer
- Source: tc_7_2_3_26:lt_TxAndRx LINE 16
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 2634
- Timestamp: 21:06:45:541_0
- RFN: 3159
- Chip: 20224
- Event: Repeat
- Source: tc_7_2_3_26:lt_TimerStatusPeriodicTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2639
- Timestamp: 21:06:45:560_1
- RFN: 3161
- Chip: 17664
- Event: Timeout
- Source: tc_7_2_3_26:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 2659
- Timestamp: 21:06:45:601_0
- RFN: 3165
- Chip: 17408
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000010110'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '768DBE39AC3B53886BF13287BF3986'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 b1 1e 76 8d be 39 ac 3b 53 88 6b f1 32 87 bf 39 86

- No.: 2668
- Timestamp: 21:06:45:614_1
- RFN: 3166
- Chip: 31232
- Event: Start Timer
- Source: tc_7_2_3_26:lt_TxAndRx LINE 16
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 2669
- Timestamp: 21:06:45:614_2
- RFN: 3166
- Chip: 32000
- Event: Repeat
- Source: tc_7_2_3_26:lt_TimerStatusPeriodicTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2674
- Timestamp: 21:06:45:634_1
- RFN: 3168
- Chip: 29952
- Event: Timeout
- Source: tc_7_2_3_26:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 2694
- Timestamp: 21:06:45:674_0
- RFN: 3172
- Chip: 29696
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000010111'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '95BDC635ADC49F43207AA6EF1B292E'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 b9 1e 95 bd c6 35 ad c4 9f 43 20 7a a6 ef 1b 29 2e

- No.: 2703
- Timestamp: 21:06:45:687_1
- RFN: 3174
- Chip: 4352
- Event: Start Timer
- Source: tc_7_2_3_26:lt_TxAndRx LINE 16
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 2704
- Timestamp: 21:06:45:687_2
- RFN: 3174
- Chip: 5376
- Event: Repeat
- Source: tc_7_2_3_26:lt_TimerStatusPeriodicTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2709
- Timestamp: 21:06:45:713_0
- RFN: 3176
- Chip: 26880
- Event: Timeout
- Source: tc_7_2_3_26:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 2729
- Timestamp: 21:06:45:753_0
- RFN: 3180
- Chip: 28928
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000011000'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '84EA1BA93BD39D3C8615A891428AEB'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 c1 1e 84 ea 1b a9 3b d3 9d 3c 86 15 a8 91 42 8a eb

- No.: 2738
- Timestamp: 21:06:45:767_0
- RFN: 3182
- Chip: 4352
- Event: Start Timer
- Source: tc_7_2_3_26:lt_TxAndRx LINE 16
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 2739
- Timestamp: 21:06:45:767_1
- RFN: 3182
- Chip: 5120
- Event: Repeat
- Source: tc_7_2_3_26:lt_TimerStatusPeriodicTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2744
- Timestamp: 21:06:45:779_1
- RFN: 3183
- Chip: 12544
- Event: Timeout
- Source: tc_7_2_3_26:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 2764
- Timestamp: 21:06:45:819_0
- RFN: 3187
- Chip: 13824
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000011001'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'B1382C04AA110280400AABBB939797'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 c9 1e b1 38 2c 04 aa 11 02 80 40 0a ab bb 93 97 97

- No.: 2773
- Timestamp: 21:06:45:833_0
- RFN: 3188
- Chip: 27648
- Event: Start Timer
- Source: tc_7_2_3_26:lt_TxAndRx LINE 16
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 2774
- Timestamp: 21:06:45:833_1
- RFN: 3188
- Chip: 28672
- Event: Repeat
- Source: tc_7_2_3_26:lt_TimerStatusPeriodicTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2779
- Timestamp: 21:06:45:845_1
- RFN: 3189
- Chip: 37120
- Event: Timeout
- Source: tc_7_2_3_26:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 2799
- Timestamp: 21:06:45:889_0
- RFN: 3194
- Chip: 9984
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000011010'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '3D863F067F0CD4B74720D01D562250'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 d1 1e 3d 86 3f 06 7f 0c d4 b7 47 20 d0 1d 56 22 50

- No.: 2808
- Timestamp: 21:06:45:902_1
- RFN: 3195
- Chip: 23552
- Event: Start Timer
- Source: tc_7_2_3_26:lt_TxAndRx LINE 16
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 2809
- Timestamp: 21:06:45:903_0
- RFN: 3195
- Chip: 24576
- Event: Repeat
- Source: tc_7_2_3_26:lt_TimerStatusPeriodicTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2812
- Timestamp: 21:06:45:908_0
- RFN: 3196
- Chip: 7680
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_26:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. STATUS_PDU
. . (DC_Field)dC_Field[1] = '0'B
. . (CtrlPDU_Type)type[3] = '000'B
. . SuperFields
. . (HexStringType)superFieldsAndPadRx[35] = '20180000000000000000000000000000000'H
. . (Padding)paddingTx[0] = -
- Constraint:
car_StatusInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 02 01 80 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00

- No.: 2815
- Timestamp: 21:06:45:914_1
- RFN: 3196
- Chip: 30208
- Event: Repeat
- Source: tc_7_2_3_26:lt_TimerStatusPeriodicTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2820
- Timestamp: 21:06:45:921_1
- RFN: 3197
- Chip: 19200
- Event: Timeout
- Source: tc_7_2_3_26:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 2840
- Timestamp: 21:06:45:962_0
- RFN: 3201
- Chip: 21248
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000011011'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '5D5C89EBCECB1ED648F418A94420AF'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 d9 1e 5d 5c 89 eb ce cb 1e d6 48 f4 18 a9 44 20 af

- No.: 2849
- Timestamp: 21:06:45:975_1
- RFN: 3202
- Chip: 35584
- Event: Start Timer
- Source: tc_7_2_3_26:lt_TxAndRx LINE 16
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 2850
- Timestamp: 21:06:45:976_0
- RFN: 3202
- Chip: 36608
- Event: Repeat
- Source: tc_7_2_3_26:lt_TimerStatusPeriodicTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2855
- Timestamp: 21:06:45:988_1
- RFN: 3204
- Chip: 7680
- Event: Timeout
- Source: tc_7_2_3_26:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 2875
- Timestamp: 21:06:46:029_0
- RFN: 3208
- Chip: 11008
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000011100'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'EE64F0B2B846A0EFE4CF4B212FD19D'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 e1 1e ee 64 f0 b2 b8 46 a0 ef e4 cf 4b 21 2f d1 9d

- No.: 2884
- Timestamp: 21:06:46:042_1
- RFN: 3209
- Chip: 25088
- Event: Start Timer
- Source: tc_7_2_3_26:lt_TxAndRx LINE 16
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 2885
- Timestamp: 21:06:46:043_0
- RFN: 3209
- Chip: 26368
- Event: Repeat
- Source: tc_7_2_3_26:lt_TimerStatusPeriodicTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2890
- Timestamp: 21:06:46:064_1
- RFN: 3211
- Chip: 33280
- Event: Timeout
- Source: tc_7_2_3_26:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 2910
- Timestamp: 21:06:46:105_0
- RFN: 3215
- Chip: 36352
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000011101'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '69DBC9342DFB66DA490BD4620FAB3B'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 e9 1e 69 db c9 34 2d fb 66 da 49 0b d4 62 0f ab 3b

- No.: 2919
- Timestamp: 21:06:46:119_0
- RFN: 3217
- Chip: 13312
- Event: Start Timer
- Source: tc_7_2_3_26:lt_TxAndRx LINE 16
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 2920
- Timestamp: 21:06:46:119_1
- RFN: 3217
- Chip: 14336
- Event: Repeat
- Source: tc_7_2_3_26:lt_TimerStatusPeriodicTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2925
- Timestamp: 21:06:46:138_1
- RFN: 3219
- Chip: 9472
- Event: Timeout
- Source: tc_7_2_3_26:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 2945
- Timestamp: 21:06:46:178_0
- RFN: 3223
- Chip: 11264
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000011110'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '86C0E01AA9117D7372D8495E89BE93'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 f1 1e 86 c0 e0 1a a9 11 7d 73 72 d8 49 5e 89 be 93

- No.: 2954
- Timestamp: 21:06:46:193_0
- RFN: 3224
- Chip: 25344
- Event: Start Timer
- Source: tc_7_2_3_26:lt_TxAndRx LINE 16
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 2955
- Timestamp: 21:06:46:193_1
- RFN: 3224
- Chip: 26880
- Event: Repeat
- Source: tc_7_2_3_26:lt_TimerStatusPeriodicTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2960
- Timestamp: 21:06:46:215_1
- RFN: 3226
- Chip: 33536
- Event: Timeout
- Source: tc_7_2_3_26:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 2980
- Timestamp: 21:06:46:256_0
- RFN: 3231
- Chip: 512
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000011111'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '17826AF118295177D8C94BDEC9B438'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 f9 1e 17 82 6a f1 18 29 51 77 d8 c9 4b de c9 b4 38

- No.: 2989
- Timestamp: 21:06:46:273_0
- RFN: 3232
- Chip: 25344
- Event: Start Timer
- Source: tc_7_2_3_26:lt_TxAndRx LINE 16
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 2990
- Timestamp: 21:06:46:273_1
- RFN: 3232
- Chip: 26624
- Event: Repeat
- Source: tc_7_2_3_26:lt_TimerStatusPeriodicTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2993
- Timestamp: 21:06:46:279_0
- RFN: 3233
- Chip: 9728
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_26:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. STATUS_PDU
. . (DC_Field)dC_Field[1] = '0'B
. . (CtrlPDU_Type)type[3] = '000'B
. . SuperFields
. . (HexStringType)superFieldsAndPadRx[35] = '201D0000000000000000000000000000000'H
. . (Padding)paddingTx[0] = -
- Constraint:
car_StatusInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 02 01 d0 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00

- No.: 2996
- Timestamp: 21:06:46:284_1
- RFN: 3233
- Chip: 30976
- Event: Repeat
- Source: tc_7_2_3_26:lt_TimerStatusPeriodicTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3001
- Timestamp: 21:06:46:290_0
- RFN: 3234
- Chip: 13568
- Event: Timeout
- Source: tc_7_2_3_26:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 3021
- Timestamp: 21:06:46:331_0
- RFN: 3238
- Chip: 18944
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000100000'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'AC11FD6625AF6E71A7C59F698E94E8'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 01 1e ac 11 fd 66 25 af 6e 71 a7 c5 9f 69 8e 94 e8

- No.: 3030
- Timestamp: 21:06:46:344_1
- RFN: 3239
- Chip: 32768
- Event: Start Timer
- Source: tc_7_2_3_26:lt_TxAndRx LINE 16
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 3031
- Timestamp: 21:06:46:345_0
- RFN: 3239
- Chip: 34048
- Event: Repeat
- Source: tc_7_2_3_26:lt_TimerStatusPeriodicTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3036
- Timestamp: 21:06:46:373_1
- RFN: 3242
- Chip: 27392
- Event: Timeout
- Source: tc_7_2_3_26:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 3056
- Timestamp: 21:06:46:414_0
- RFN: 3246
- Chip: 30464
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000100001'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'B147DF3678F3E79A690E81BFC660F0'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 09 1e b1 47 df 36 78 f3 e7 9a 69 0e 81 bf c6 60 f0

- No.: 3065
- Timestamp: 21:06:46:427_1
- RFN: 3248
- Chip: 7424
- Event: Start Timer
- Source: tc_7_2_3_26:lt_TxAndRx LINE 16
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 3066
- Timestamp: 21:06:46:428_0
- RFN: 3248
- Chip: 8192
- Event: Repeat
- Source: tc_7_2_3_26:lt_TimerStatusPeriodicTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3071
- Timestamp: 21:06:46:450_1
- RFN: 3250
- Chip: 16896
- Event: Timeout
- Source: tc_7_2_3_26:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 3091
- Timestamp: 21:06:46:490_0
- RFN: 3254
- Chip: 19712
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000100010'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '1803FF9996971728D148215022AFBB'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 11 1e 18 03 ff 99 96 97 17 28 d1 48 21 50 22 af bb

- No.: 3100
- Timestamp: 21:06:46:505_1
- RFN: 3255
- Chip: 33792
- Event: Start Timer
- Source: tc_7_2_3_26:lt_TxAndRx LINE 16
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 3101
- Timestamp: 21:06:46:505_2
- RFN: 3255
- Chip: 35072
- Event: Repeat
- Source: tc_7_2_3_26:lt_TimerStatusPeriodicTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3106
- Timestamp: 21:06:46:520_1
- RFN: 3257
- Chip: 14336
- Event: Timeout
- Source: tc_7_2_3_26:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 3126
- Timestamp: 21:06:46:561_0
- RFN: 3261
- Chip: 18944
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000100011'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '392C2E04FF4CDE1CFCB3478A6BA46F'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 19 1e 39 2c 2e 04 ff 4c de 1c fc b3 47 8a 6b a4 6f

- No.: 3135
- Timestamp: 21:06:46:575_1
- RFN: 3262
- Chip: 34816
- Event: Start Timer
- Source: tc_7_2_3_26:lt_TxAndRx LINE 16
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 3136
- Timestamp: 21:06:46:575_2
- RFN: 3262
- Chip: 35584
- Event: Repeat
- Source: tc_7_2_3_26:lt_TimerStatusPeriodicTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3141
- Timestamp: 21:06:46:589_1
- RFN: 3264
- Chip: 11776
- Event: Timeout
- Source: tc_7_2_3_26:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 3161
- Timestamp: 21:06:46:630_0
- RFN: 3268
- Chip: 16640
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000100100'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '5B23853F798C3E0655A23AF9197C26'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 21 1e 5b 23 85 3f 79 8c 3e 06 55 a2 3a f9 19 7c 26

- No.: 3170
- Timestamp: 21:06:46:644_0
- RFN: 3269
- Chip: 30976
- Event: Start Timer
- Source: tc_7_2_3_26:lt_TxAndRx LINE 16
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 3171
- Timestamp: 21:06:46:644_1
- RFN: 3269
- Chip: 32000
- Event: Repeat
- Source: tc_7_2_3_26:lt_TimerStatusPeriodicTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3176
- Timestamp: 21:06:46:658_1
- RFN: 3271
- Chip: 8448
- Event: Timeout
- Source: tc_7_2_3_26:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 3196
- Timestamp: 21:06:46:702_0
- RFN: 3275
- Chip: 23296
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000100101'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '05AA3BAC6E0E54F74D8B6B8EC1B56D'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 29 1e 05 aa 3b ac 6e 0e 54 f7 4d 8b 6b 8e c1 b5 6d

- No.: 3205
- Timestamp: 21:06:46:716_0
- RFN: 3277
- Chip: 1280
- Event: Start Timer
- Source: tc_7_2_3_26:lt_TxAndRx LINE 16
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 3206
- Timestamp: 21:06:46:716_1
- RFN: 3277
- Chip: 2304
- Event: Repeat
- Source: tc_7_2_3_26:lt_TimerStatusPeriodicTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3209
- Timestamp: 21:06:46:722_0
- RFN: 3277
- Chip: 23552
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_26:lt_TxAndRx LINE 4
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. STATUS_PDU
. . (DC_Field)dC_Field[1] = '0'B
. . (CtrlPDU_Type)type[3] = '000'B
. . SuperFields
. . (HexStringType)superFieldsAndPadRx[35] = '20230000000000000000000000000000000'H
. . (Padding)paddingTx[0] = -
- Constraint:
car_StatusInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 02 02 30 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00

- No.: 3212
- Timestamp: 21:06:46:728_1
- RFN: 3278
- Chip: 9984
- Event: Repeat
- Source: tc_7_2_3_26:lt_TimerStatusPeriodicTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3215
- Timestamp: 21:06:46:731_0
- RFN: 3278
- Chip: 19712
- Event: Timeout
- Source: tc_7_2_3_26:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 3235
- Timestamp: 21:06:46:771_0
- RFN: 3282
- Chip: 22784
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000100110'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'DB638F94C21FA991682405FF6670F2'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 31 1e db 63 8f 94 c2 1f a9 91 68 24 05 ff 66 70 f2

- No.: 3244
- Timestamp: 21:06:46:785_1
- RFN: 3283
- Chip: 36864
- Event: Start Timer
- Source: tc_7_2_3_26:lt_TxAndRx LINE 16
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 3245
- Timestamp: 21:06:46:785_2
- RFN: 3283
- Chip: 37888
- Event: Repeat
- Source: tc_7_2_3_26:lt_TimerStatusPeriodicTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3250
- Timestamp: 21:06:46:796_1
- RFN: 3285
- Chip: 2560
- Event: Timeout
- Source: tc_7_2_3_26:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 3270
- Timestamp: 21:06:46:838_0
- RFN: 3289
- Chip: 5632
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000100111'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'B2ED1B7C735876A710D7E2650F7E73'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 39 1e b2 ed 1b 7c 73 58 76 a7 10 d7 e2 65 0f 7e 73

- No.: 3279
- Timestamp: 21:06:46:851_1
- RFN: 3290
- Chip: 19968
- Event: Start Timer
- Source: tc_7_2_3_26:lt_TxAndRx LINE 16
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 3282
- Timestamp: 21:06:46:855_1
- RFN: 3290
- Chip: 33024
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: tc_7_2_3_26:lt_CheckNumStatus LINE 1
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3287
- Timestamp: 21:06:46:864_1
- RFN: 3291
- Chip: 32000
- Event: Cancel Timer
- Source: tc_7_2_3_26:lt_TimerStatusPeriodicTest LINE 11
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 3289
- Timestamp: 21:06:46:868_1
- RFN: 3292
- Chip: 8192
- Event: Cancel Timer
- Source: tc_7_2_3_26:lt_TimerStatusPeriodicTest LINE 12
- Message Structure:
no details available
- Constraint:
t_Status
- BinaryMessage:

- No.: 3298
- Timestamp: 21:06:46:873_0
- RFN: 3292
- Chip: 26112
- Event: Send
- PCO: Dc
- Message: RRC_DataReq
- Source: ts_TC_DeactivateRB_TestMode LINE 6
- Message Structure:
RRC_DataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[-1] = -
. (SapId)sapId[1] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. DEACTIVATERBTESTMODE
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)tCProtocolDiscriminator[4] = '1111'B
. . (MsgType)msgType[8] = '01000110'B
- Constraint:
ca_PS_DataReq
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 0f 46

- No.: 3299
- Timestamp: 21:06:46:874_0
- RFN: 3292
- Chip: 29440
- Event: Start Timer
- Source: ts_TC_DeactivateRB_TestMode LINE 6
- Message Structure:
no details available
- Constraint:
t_Dly (5000 Ms)
- BinaryMessage:

- No.: 3306
- Timestamp: 21:06:47:167_0
- RFN: 3322
- Chip: 4608
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_TC_DeactivateRB_TestMode LINE 7
- Message Structure:
RRC_DataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. (START_Value)start[0] = -
. DEACTIVATERBTESTMODECOMPLETE
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)tCProtocolDiscriminator[4] = '1111'B
. . (MsgType)msgType[8] = '01000111'B
- Constraint:
car_PS_UplinkDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 0f 47

- No.: 3307
- Timestamp: 21:06:47:168_0
- RFN: 3322
- Chip: 8448
- Event: Cancel Timer
- Source: ts_TC_DeactivateRB_TestMode LINE 7
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 3308
- Timestamp: 21:06:47:169_0
- RFN: 3322
- Chip: 9216
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_TC_DeactivateRB_TestMode LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3320
- Timestamp: 21:06:47:176_0
- RFN: 3322
- Chip: 37632
- Event: Send
- PCO: UM
- Message: RLC_UM_DATA_REQ
- Source: po_ConnectionAndSS_Rel:lt_Send_RRC_ConnectionRelease LINE 8
- Message Structure:
RLC_UM_DATA_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. uM_message
. . DL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00000000000000000000000000000000"
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . DL_DCCH_MessageType
. . . . RRCConnectionRelease
. . . . . r3
. . . . . . RRCConnectionRelease_r3_IEs
. . . . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . . . (IntegerType)n_308 = 1
. . . . . . . (ReleaseCause)releaseCause = 0
. . . . . . . Rplmn_Information
. . . . . . laterNonCriticalExtensions
. (BooleanType)specialLI = FALSE
- Constraint:
cas_RRC_ConnRelDCCH
- BinaryMessage:
30 10 02 01 ff 02 01 01 80 00 00 00 03 c8 00 01 01 00

- No.: 3322
- Timestamp: 21:06:47:179_0
- RFN: 3323
- Chip: 11520
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: RRC_Def1 LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. STATUS_PDU
. . (DC_Field)dC_Field[1] = '0'B
. . (CtrlPDU_Type)type[3] = '000'B
. . SuperFields
. . (HexStringType)superFieldsAndPadRx[35] = '20280000000000000000000000000000000'H
. . (Padding)paddingTx[0] = -
- Constraint:
car_StatusInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 02 02 80 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00

- No.: 3323
- Timestamp: 21:06:47:180_0
- RFN: 3323
- Chip: 14848
- Event: Default
- Source: RRC_Def1 LINE 0
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3324
- Timestamp: 21:06:47:180_1
- RFN: 3323
- Chip: 15616
- Event: Default
- Source: po_ConnectionAndSS_Rel:lt_Send_RRC_ConnectionRelease LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3329
- Timestamp: 21:06:47:408_0
- RFN: 3346
- Chip: 10240
- Event: Receive
- PCO: UM
- Message: RLC_UM_DATA_IND
- Source: po_ConnectionAndSS_Rel:lt_Send_RRC_ConnectionRelease LINE 9
- Message Structure:
RLC_UM_DATA_IND
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. IntegrityResult
. uM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "10110011101011111111101100111000"
. . . . (IntegerType)rrc_MessageSequenceNumber = 1
. . . UL_DCCH_MessageType
. . . . RRCConnectionReleaseComplete
. . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . FailureCauseWithProtErr
. . . . . laterNonCriticalExtensions
. . . . . . (BitStringType)rrcConnectionReleaseComplete_r3_add_ext = 0
. . . . . . nonCriticalExtensions
- Constraint:
car_RRC_ConnRelCmplUM
- BinaryMessage:
30 0c 02 01 ff 02 01 01 d9 d7 fd 9c 0c 40

- No.: 3330
- Timestamp: 21:06:47:409_0
- RFN: 3346
- Chip: 14592
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: po_ConnectionAndSS_Rel:lt_Send_RRC_ConnectionRelease LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3333
- Timestamp: 21:06:47:410_2
- RFN: 3346
- Chip: 19200
- Event: Start Timer
- Source: po_ConnectionAndSS_Rel:lt_RptRcvConnRel LINE 1
- Message Structure:
no details available
- Constraint:
t_Dly (5000 Ms)
- BinaryMessage:

- No.: 3338
- Timestamp: 21:06:47:467_0
- RFN: 3352
- Chip: 2560
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: RRC_Def1 LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. STATUS_PDU
. . (DC_Field)dC_Field[1] = '0'B
. . (CtrlPDU_Type)type[3] = '000'B
. . SuperFields
. . (HexStringType)superFieldsAndPadRx[35] = '20280000000000000000000000000000000'H
. . (Padding)paddingTx[0] = -
- Constraint:
car_StatusInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 02 02 80 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00

- No.: 3339
- Timestamp: 21:06:47:468_0
- RFN: 3352
- Chip: 5888
- Event: Default
- Source: RRC_Def1 LINE 0
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3340
- Timestamp: 21:06:47:468_1
- RFN: 3352
- Chip: 6656
- Event: Default
- Source: po_ConnectionAndSS_Rel:lt_RptRcvConnRel LINE 4
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3345
- Timestamp: 21:06:47:568_0
- RFN: 3362
- Chip: 8192
- Event: Receive
- PCO: UM
- Message: RLC_UM_DATA_IND
- Source: po_ConnectionAndSS_Rel:lt_RptRcvConnRel LINE 4
- Message Structure:
RLC_UM_DATA_IND
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. IntegrityResult
. uM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00111001011111110001011000001001"
. . . . (IntegerType)rrc_MessageSequenceNumber = 2
. . . UL_DCCH_MessageType
. . . . RRCConnectionReleaseComplete
. . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . FailureCauseWithProtErr
. . . . . laterNonCriticalExtensions
. . . . . . (BitStringType)rrcConnectionReleaseComplete_r3_add_ext = 0
. . . . . . nonCriticalExtensions
- Constraint:
car_RRC_ConnRelCmplUM
- BinaryMessage:
30 0c 02 01 ff 02 01 01 9c bf 8b 04 94 40

- No.: 3346
- Timestamp: 21:06:47:569_0
- RFN: 3362
- Chip: 12544
- Event: Cancel Timer
- Source: po_ConnectionAndSS_Rel:lt_RptRcvConnRel LINE 4
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 3347
- Timestamp: 21:06:47:569_1
- RFN: 3362
- Chip: 13568
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: po_ConnectionAndSS_Rel:lt_RptRcvConnRel LINE 4
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3363
- Timestamp: 21:06:47:576_0
- RFN: 3363
- Chip: 0
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 01 0a 01 00 05 00

- No.: 3367
- Timestamp: 21:06:47:585_0
- RFN: 3363
- Chip: 35840
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 3370
- Timestamp: 21:06:47:588_0
- RFN: 3364
- Chip: 7680
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 02 0a 01 00 05 00

- No.: 3374
- Timestamp: 21:06:47:597_0
- RFN: 3365
- Chip: 5120
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 3377
- Timestamp: 21:06:47:600_0
- RFN: 3365
- Chip: 16384
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 03 0a 01 00 05 00

- No.: 3381
- Timestamp: 21:06:47:611_0
- RFN: 3366
- Chip: 19200
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 3384
- Timestamp: 21:06:47:614_0
- RFN: 3366
- Chip: 30208
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 04 0a 01 00 05 00

- No.: 3388
- Timestamp: 21:06:47:624_0
- RFN: 3367
- Chip: 31232
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 3394
- Timestamp: 21:06:47:628_0
- RFN: 3368
- Chip: 7424
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = -12
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 f4 0a 01 00 05 00

- No.: 3398
- Timestamp: 21:06:47:635_0
- RFN: 3368
- Chip: 34560
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = -12
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 f4

- No.: 3402
- Timestamp: 21:06:47:644_0
- RFN: 3369
- Chip: 30976
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_CMAC_Rel LINE 1
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
. (RatType)ratType = 0
. configMessage
- Constraint:
cas_MAC_Rel
- BinaryMessage:
30 0b 02 01 ff 02 01 1a 0a 01 00 05 00

- No.: 3406
- Timestamp: 21:06:47:648_0
- RFN: 3370
- Chip: 9728
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_CMAC_Rel LINE 2
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 1a

- No.: 3409
- Timestamp: 21:06:47:655_0
- RFN: 3370
- Chip: 34560
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_CMAC_Rel LINE 1
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
. (RatType)ratType = 0
. configMessage
- Constraint:
cas_MAC_Rel
- BinaryMessage:
30 0b 02 01 ff 02 01 14 0a 01 00 05 00

- No.: 3413
- Timestamp: 21:06:47:662_0
- RFN: 3371
- Chip: 24320
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_CMAC_Rel LINE 2
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 14

- No.: 3416
- Timestamp: 21:06:47:664_0
- RFN: 3371
- Chip: 34048
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Release_REQ
- Source: ts_CPHY_TrChRel LINE 1
- Message Structure:
CPHY_TrCH_Release_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
ca_PHY_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 1a

- No.: 3421
- Timestamp: 21:06:47:674_0
- RFN: 3372
- Chip: 32512
- Event: Receive
- PCO: CPHY
- Message: CPHY_Out_of_Sync_IND
- Source: SS_Def LINE 5
- Message Structure:
CPHY_Out_of_Sync_IND
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_OutOfSyncInd
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 3422
- Timestamp: 21:06:47:676_0
- RFN: 3373
- Chip: 2304
- Event: Default
- Source: SS_Def LINE 0
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3423
- Timestamp: 21:06:47:676_1
- RFN: 3373
- Chip: 3072
- Event: Default
- Source: ts_CPHY_TrChRel LINE 2
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3425
- Timestamp: 21:06:47:678_0
- RFN: 3373
- Chip: 10496
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Release_CNF
- Source: ts_CPHY_TrChRel LINE 2
- Message Structure:
CPHY_TrCH_Release_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
ca_PHY_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 1a

- No.: 3428
- Timestamp: 21:06:47:681_0
- RFN: 3373
- Chip: 21248
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Release_REQ
- Source: ts_CPHY_TrChRel LINE 1
- Message Structure:
CPHY_TrCH_Release_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_PHY_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 3432
- Timestamp: 21:06:47:708_0
- RFN: 3376
- Chip: 8960
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Release_CNF
- Source: ts_CPHY_TrChRel LINE 2
- Message Structure:
CPHY_TrCH_Release_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_PHY_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 3435
- Timestamp: 21:06:47:711_0
- RFN: 3376
- Chip: 19968
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 1a

- No.: 3439
- Timestamp: 21:06:47:718_0
- RFN: 3377
- Chip: 10752
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 1a

- No.: 3442
- Timestamp: 21:06:47:721_0
- RFN: 3377
- Chip: 21760
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 3446
- Timestamp: 21:06:47:747_0
- RFN: 3380
- Chip: 8192
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 3451
- Timestamp: 21:06:47:751_0
- RFN: 3380
- Chip: 21504
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 00 02 01 00 0a 01 00 05 00

- No.: 3455
- Timestamp: 21:06:47:757_0
- RFN: 3381
- Chip: 4864
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 00

- No.: 3458
- Timestamp: 21:06:47:762_0
- RFN: 3381
- Chip: 22272
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_CMAC_Rel LINE 1
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 8
. (RatType)ratType = 0
. configMessage
- Constraint:
cas_MAC_Rel
- BinaryMessage:
30 0b 02 01 00 02 01 08 0a 01 00 05 00

- No.: 3462
- Timestamp: 21:06:47:766_0
- RFN: 3382
- Chip: 0
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_CMAC_Rel LINE 2
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 8
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 08

- No.: 3465
- Timestamp: 21:06:47:769_0
- RFN: 3382
- Chip: 10496
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Release_REQ
- Source: ts_CPHY_TrChRel LINE 1
- Message Structure:
CPHY_TrCH_Release_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 8
- Constraint:
ca_PHY_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 08

- No.: 3469
- Timestamp: 21:06:47:796_0
- RFN: 3384
- Chip: 37632
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Release_CNF
- Source: ts_CPHY_TrChRel LINE 2
- Message Structure:
CPHY_TrCH_Release_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 8
- Constraint:
ca_PHY_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 08

- No.: 3472
- Timestamp: 21:06:47:799_0
- RFN: 3385
- Chip: 9728
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 7
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 07

- No.: 3476
- Timestamp: 21:06:47:804_0
- RFN: 3385
- Chip: 30976
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 7
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 07

- No.: 3479
- Timestamp: 21:06:47:807_0
- RFN: 3386
- Chip: 2816
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 8
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 08

- No.: 3483
- Timestamp: 21:06:47:834_0
- RFN: 3388
- Chip: 32000
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 8
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 08

- No.: 3486
- Timestamp: 21:06:47:837_0
- RFN: 3389
- Chip: 4864
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -2
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 00 02 01 fe 0a 01 00 05 00

- No.: 3490
- Timestamp: 21:06:47:843_0
- RFN: 3389
- Chip: 27136
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 fe

- No.: 3493
- Timestamp: 21:06:47:847_0
- RFN: 3390
- Chip: 4096
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_CMAC_Rel LINE 1
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 5
. (RatType)ratType = 0
. configMessage
- Constraint:
cas_MAC_Rel
- BinaryMessage:
30 0b 02 01 00 02 01 05 0a 01 00 05 00

- No.: 3497
- Timestamp: 21:06:47:853_0
- RFN: 3390
- Chip: 28160
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_CMAC_Rel LINE 2
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 5
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 05

- No.: 3500
- Timestamp: 21:06:47:856_0
- RFN: 3391
- Chip: 512
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Release_REQ
- Source: ts_CPHY_TrChRel LINE 1
- Message Structure:
CPHY_TrCH_Release_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 5
- Constraint:
ca_PHY_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 05

- No.: 3504
- Timestamp: 21:06:47:863_0
- RFN: 3391
- Chip: 27904
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Release_CNF
- Source: ts_CPHY_TrChRel LINE 2
- Message Structure:
CPHY_TrCH_Release_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 5
- Constraint:
ca_PHY_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 05

- No.: 3507
- Timestamp: 21:06:47:866_0
- RFN: 3392
- Chip: 0
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 6
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 06

- No.: 3511
- Timestamp: 21:06:47:873_0
- RFN: 3392
- Chip: 27136
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 6
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 06

- No.: 3514
- Timestamp: 21:06:47:876_0
- RFN: 3392
- Chip: 37888
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 5
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 05

- No.: 3518
- Timestamp: 21:06:47:884_0
- RFN: 3393
- Chip: 30720
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 5
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 05

- No.: 3523
- Timestamp: 21:06:47:887_0
- RFN: 3394
- Chip: 5632
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 00 02 01 ff 0a 01 00 05 00

- No.: 3527
- Timestamp: 21:06:47:892_0
- RFN: 3394
- Chip: 24064
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 3530
- Timestamp: 21:06:47:895_0
- RFN: 3394
- Chip: 36864
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_CMAC_Rel LINE 1
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 4
. (RatType)ratType = 0
. configMessage
- Constraint:
cas_MAC_Rel
- BinaryMessage:
30 0b 02 01 00 02 01 04 0a 01 00 05 00

- No.: 3534
- Timestamp: 21:06:47:902_0
- RFN: 3395
- Chip: 24064
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_CMAC_Rel LINE 2
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 4
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 04

- No.: 3537
- Timestamp: 21:06:47:905_0
- RFN: 3395
- Chip: 34560
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Release_REQ
- Source: ts_CPHY_TrChRel LINE 1
- Message Structure:
CPHY_TrCH_Release_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 4
- Constraint:
ca_PHY_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 04

- No.: 3541
- Timestamp: 21:06:47:911_0
- RFN: 3396
- Chip: 19712
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Release_CNF
- Source: ts_CPHY_TrChRel LINE 2
- Message Structure:
CPHY_TrCH_Release_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 4
- Constraint:
ca_PHY_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 04

- No.: 3544
- Timestamp: 21:06:47:914_0
- RFN: 3396
- Chip: 30208
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 2
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 02

- No.: 3548
- Timestamp: 21:06:47:919_0
- RFN: 3397
- Chip: 14080
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 2
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 02

- No.: 3551
- Timestamp: 21:06:47:922_0
- RFN: 3397
- Chip: 23808
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 1
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 01

- No.: 3555
- Timestamp: 21:06:47:928_0
- RFN: 3398
- Chip: 10496
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 1
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 01

- No.: 3558
- Timestamp: 21:06:47:931_0
- RFN: 3398
- Chip: 21248
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 4
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 04

- No.: 3562
- Timestamp: 21:06:47:938_0
- RFN: 3399
- Chip: 8960
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 4
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 04

- No.: 3565
- Timestamp: 21:06:47:941_0
- RFN: 3399
- Chip: 19200
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 0
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 00

- No.: 3569
- Timestamp: 21:06:47:946_0
- RFN: 3400
- Chip: 1536
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 0
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 00

- No.: 3586
- Timestamp: 21:06:47:964_0
- RFN: 3401
- Chip: 33024
- Event: Log
- PCO: VERDICT
- Message: PASS
- Source: tc_7_2_3_26 LINE 4
- Message Structure:
no details available
- Constraint:
- BinaryMessage: