- No.: 2
- Timestamp: 20:28:20:120_0
- RFN: 3045
- Chip: 22016
- Event: Start Timer
- Source: tc_7_2_2_6 LINE 1
- Message Structure:
no details available
- Constraint:
t_Guard (300 Sec)
- BinaryMessage:

- No.: 88
- Timestamp: 20:28:20:153_0
- RFN: 3048
- Chip: 30720
- Event: Send
- PCO: Ut
- Message: MMI_CmdReq
- Source: ts_MMI_UE_SwitchOff LINE 1
- Message Structure:
MMI_CmdReq
. (IA5StringType)cmd[-1] = "Please switch off the UE"
- Constraint:
ca_MMI_CmdReq
- BinaryMessage:
50 6c 65 61 73 65 20 73 77 69 74 63 68 20 6f 66 66 20 20 74 68 65 20 55 45

- No.: 92
- Timestamp: 20:28:22:332_0
- RFN: 3266
- Chip: 25856
- Event: Receive
- PCO: Ut
- Message: MMI_CmdCnf
- Source: ts_MMI_UE_SwitchOff LINE 2
- Message Structure:
MMI_CmdCnf
. (BooleanType)result = TRUE
. (IA5StringType)resultString[6] = " OK "
- Constraint:
ca_MMI_CmdCnf
- BinaryMessage:
80 0d 0a 4f 4b 0d 0a

- No.: 96
- Timestamp: 20:28:22:334_0
- RFN: 3266
- Chip: 35328
- Event: Send
- PCO: CPHY
- Message: CPHY_Ini_REQ
- Source: ts_SS_CellCfg:lt_CelllsAlreadyStarted LINE 5
- Message Structure:
CPHY_Ini_REQ
. (CPHY_Ini_REQ)CPHY_Ini_REQ = 0
- Constraint:
cas_InitReqDef
- BinaryMessage:
0a 01 00

- No.: 100
- Timestamp: 20:28:24:383_0
- RFN: 10
- Chip: 14080
- Event: Receive
- PCO: CPHY
- Message: CPHY_Ini_CNF
- Source: ts_SS_CellCfg:lt_CelllsAlreadyStarted LINE 6
- Message Structure:
CPHY_Ini_CNF
- Constraint:
car_IniCnf
- BinaryMessage:
30 02 05 00

- No.: 104
- Timestamp: 20:28:24:387_0
- RFN: 10
- Chip: 25856
- Event: Send
- PCO: CPHY
- Message: CPHY_Cell_Config_REQ
- Source: ts_SS_CellCfg LINE 6
- Message Structure:
CPHY_Cell_Config_REQ
. (IntegerType)cellId = 0
. (IntegerType)tcell = 0
. (IntegerType)sfnOffset = 0
. FrequencyInfo
. . modeSpecificInfo
. . . FrequencyInfoFDD
. . . . (IntegerType)uarfcn_UL = -
. . . . (IntegerType)uarfcn_DL = 10700
. (IntegerType)primaryScramblingCode_SS = 100
. CellTxPowerLevel
. (IntegerType)dLTxAttenuationLevel = 0
- Constraint:
ca_CellCfgReq
- BinaryMessage:
30 19 02 01 00 02 01 00 02 01 00 30 06 30 04 02 02 29 cc 02 01 64 05 00 02 01 00

- No.: 108
- Timestamp: 20:28:25:296_0
- RFN: 101
- Chip: 25088
- Event: Receive
- PCO: CPHY
- Message: CPHY_Cell_Config_CNF
- Source: ts_SS_CellCfg LINE 7
- Message Structure:
CPHY_Cell_Config_CNF
. (IntegerType)cellId = 0
- Constraint:
ca_CellCfgCnf
- BinaryMessage:
30 03 02 01 00

- No.: 120
- Timestamp: 20:28:25:303_0
- RFN: 102
- Chip: 11008
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 3
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 0
. (RatType)ratType = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . PrimaryCPICHInfo
. . . . (IntegerType)dl_TxPower_PCPICH = -60
. . . . (BooleanType)txdiversityIndicator = FALSE
- Constraint:
ca_pCPICH_Info
- BinaryMessage:
30 13 02 01 00 02 01 00 0a 01 00 30 08 30 06 02 01 c4 01 01 00

- No.: 124
- Timestamp: 20:28:25:308_0
- RFN: 102
- Chip: 32256
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 4
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 0
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 00

- No.: 125
- Timestamp: 20:28:25:312_0
- RFN: 103
- Chip: 6656
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 5
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 1
. (RatType)ratType = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . PrimarySCHInfo
. . . . (BooleanType)tstdIndicator = FALSE
. . . . (IntegerType)dl_TxPower = -5
- Constraint:
ca_pSCH_Info
- BinaryMessage:
30 13 02 01 00 02 01 01 0a 01 00 30 08 30 06 01 01 00 02 01 fb

- No.: 129
- Timestamp: 20:28:25:317_0
- RFN: 103
- Chip: 26368
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 6
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 1
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 01

- No.: 130
- Timestamp: 20:28:25:320_0
- RFN: 104
- Chip: 1024
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 7
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 2
. (RatType)ratType = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . SecondarySCHInfo
. . . . (BooleanType)tstdIndicator = FALSE
. . . . (IntegerType)dl_TxPower = -5
- Constraint:
ca_sSCH_Info
- BinaryMessage:
30 13 02 01 00 02 01 02 0a 01 00 30 08 30 06 01 01 00 02 01 fb

- No.: 134
- Timestamp: 20:28:25:458_0
- RFN: 117
- Chip: 32512
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 8
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 2
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 02

- No.: 135
- Timestamp: 20:28:25:461_0
- RFN: 118
- Chip: 7168
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 9
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 4
. (RatType)ratType = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . PrimaryCCPCHInfo
. . . . (BooleanType)sttd_Indicator = FALSE
. . . . (IntegerType)dl_TxPower = -2
- Constraint:
ca_pCCPCH_Info
- BinaryMessage:
30 13 02 01 00 02 01 04 0a 01 00 30 08 30 06 01 01 00 02 01 fe

- No.: 139
- Timestamp: 20:28:25:469_0
- RFN: 118
- Chip: 34048
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 10
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 4
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 04

- No.: 140
- Timestamp: 20:28:25:480_0
- RFN: 119
- Chip: 36608
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Config_REQ
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 11
- Message Structure:
CPHY_TrCH_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 4
. (RatType)ratType = 0
. CphyTrchConfigReq
. . SS_ActivationTime
. . ulconnectedTrCHList
. . TFCS
. . dlconnectedTrCHList
. . . CphyTrchConfigReq_setseq_1
. . . . (IntegerType)trchid = 11
. . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 2
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 246
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional = 0
. . . . . . (IntegerType)rateMatchingAttribute = 1
. . . . . . (CRC_Size)crc_Size = 3
. . TFCS
. . . ExplicitTFCS_Configuration
. . . . TFCS_ReconfAdd
. . . . . ctfcSize
. . . . . . ctfc2Bit
. . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . (IntegerType)ctfc2 = 0
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . fdd
. . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 11
. . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
- Constraint:
ca_BCH_InfoActNow
- BinaryMessage:
30 4c 02 01 00 02 01 04 0a 01 00 30 41 05 00 30 23 30 21 02 01 0b 0a 01 02 30 19 30 0c 30 0a 02 02 00 f6 30 02 05 00 05 00 30 09 0a 01 00 02 01 01 0a 01 03 30 18 30 30 15 30 13 02 01 00 30 0e 30 0c 30 30 03 02 01 0b 02 01 0f 02 01 00

- No.: 144
- Timestamp: 20:28:25:491_0
- RFN: 121
- Chip: 2816
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Config_CNF
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 12
- Message Structure:
CPHY_TrCH_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 4
- Constraint:
ca_TrChCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 04

- No.: 145
- Timestamp: 20:28:25:507_0
- RFN: 122
- Chip: 27392
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 13
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 4
. (RatType)ratType = 0
. configMessage
. . CmacConfigReq
. . . SS_ActivationTime
. . . UE_Info
. . . . U_RNTI
. . . . (BitStringType)c_RNTI[16] = -
. . . TrCHInfo
. . . . ulconnectedTrCHList
. . . . TFCS
. . . . dlconnectedTrCHList
. . . . . TrCHInfo_setseq_1
. . . . . . (IntegerType)trchid = 11
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 246
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional = 0
. . . . . . . . (IntegerType)rateMatchingAttribute = 1
. . . . . . . . (CRC_Size)crc_Size = 3
. . . . TFCS
. . . . . ExplicitTFCS_Configuration
. . . . . . TFCS_ReconfAdd
. . . . . . . ctfcSize
. . . . . . . . ctfc2Bit
. . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . (IntegerType)ctfc2 = 0
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 11
. . . . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . TrCH_LogCHMappingList1
. . . . ulconnectedTrCHList
. . . . dlconnectedTrCHList
. . . . . TrCH_LogCHMappingList1_setseq_1
. . . . . . (IntegerType)trchid = 11
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 2
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 0
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 1
. . . . . . . . (IntegerType)rB_Identity = -1
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_CMAC_CfgInfo
- BinaryMessage:
30 70 02 01 00 02 01 04 0a 01 00 30 65 05 00 30 00 30 3c 30 20 30 1e 02 01 0b 30 19 30 0c 30 0a 02 02 00 f6 30 02 05 00 05 00 30 09 0a 01 00 02 01 01 0a 01 03 30 18 30 30 15 30 13 02 01 00 30 0e 30 0c 30 30 03 02 01 0b 02 01 0f 02 01 00 30 21 30 1f 30 1d 02 01 0b 30 18 30 16 30 11 0a 01 00 0a 01 02 02 01 01 0a 01 00 05 00 02 01 01 02 01 ff

- No.: 149
- Timestamp: 20:28:25:514_0
- RFN: 123
- Chip: 16384
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 14
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 4
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 04

- No.: 157
- Timestamp: 20:28:25:520_0
- RFN: 124
- Chip: 1024
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_PCH_FACH_CCCH_Cfg LINE 3
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 5
. (RatType)ratType = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . SecondaryCCPCHInfo
. . . . (IntegerType)scramblingCode = 0
. . . . SF256_AndCodeNumber
. . . . . (IntegerType)sf64 = 1
. . . . (IntegerType)sCCPCHSlotFormat = 8
. . . . (IntegerType)timingOffset = 0
. . . . (PositionFixedOrFlexible)positionFixedOrFlexible = 1
. . . . (BooleanType)sttd_Indicator = FALSE
. . . . (IntegerType)dl_TxPower = -2
. . . . (IntegerType)powerOffsetOfTFCI_PO1 = 6
. . . . (IntegerType)powerOffsetOfPILOT_PO3 = 6
- Constraint:
ca_sCCPCH_Info
- BinaryMessage:
30 28 02 01 00 02 01 05 0a 01 00 30 1d 30 1b 02 01 00 02 01 01 02 01 08 02 01 00 0a 01 01 01 01 00 02 01 fe 02 01 06 02 01 06

- No.: 161
- Timestamp: 20:28:25:527_0
- RFN: 124
- Chip: 27904
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_PCH_FACH_CCCH_Cfg LINE 4
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 5
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 05

- No.: 162
- Timestamp: 20:28:25:553_0
- RFN: 127
- Chip: 12032
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Config_REQ
- Source: ts_SS_PCH_FACH_CCCH_Cfg LINE 5
- Message Structure:
CPHY_TrCH_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 5
. (RatType)ratType = 0
. CphyTrchConfigReq
. . SS_ActivationTime
. . ulconnectedTrCHList
. . TFCS
. . dlconnectedTrCHList
. . . CphyTrchConfigReq_setseq_1
. . . . (IntegerType)trchid = 12
. . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 3
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 240
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional = 0
. . . . . . (IntegerType)rateMatchingAttribute = 230
. . . . . . (CRC_Size)crc_Size = 3
. . . CphyTrchConfigReq_setseq_1
. . . . (IntegerType)trchid = 13
. . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 1
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 168
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . (IntegerType)small = 2
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional = 0
. . . . . . (IntegerType)rateMatchingAttribute = 220
. . . . . . (CRC_Size)crc_Size = 3
. . . CphyTrchConfigReq_setseq_1
. . . . (IntegerType)trchid = 14
. . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 1
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 360
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . (IntegerType)rateMatchingAttribute = 130
. . . . . . (CRC_Size)crc_Size = 3
. . TFCS
. . . ExplicitTFCS_Configuration
. . . . TFCS_ReconfAdd
. . . . . ctfcSize
. . . . . . ctfc4Bit
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 0
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 1
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 2
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 3
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 4
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 5
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 6
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 8
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . fdd
. . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 11
. . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
- Constraint:
ca_PCH_2_FACH_InfoActNow
- BinaryMessage:
30 81 e4 02 01 00 02 01 05 0a 01 00 30 81 d8 05 00 30 74 30 24 02 01 0c 0a 01 03 30 1c 30 0e 30 0c 02 02 00 f0 30 04 05 00 05 00 05 00 30 0a 0a 01 00 02 02 00 e6 0a 01 03 30 27 02 01 0d 0a 01 01 30 1f 30 11 30 0f 02 02 00 a8 30 07 05 00 05 00 02 01 02 05 00 30 0a 0a 01 00 02 02 00 dc 0a 01 03 30 23 02 01 0e 0a 01 01 30 1b 30 0e 30 0c 02 02 01 68 30 04 05 00 05 00 05 00 30 09 05 00 02 02 00 82 0a 01 03 30 5e 30 30 5b 30 08 02 01 00 30 03 02 01 00 30 08 02 01 01 30 03 02 01 00 30 08 02 01 02 30 03 02 01 00 30 08 02 01 03 30 03 02 01 00 30 08 02 01 04 30 03 02 01 00 30 08 02 01 05 30 03 02 01 00 30 08 02 01 06 30 03 02 01 00 30 13 02 01 08 30 0e 30 0c 30 30 03 02 01 0b 02 01 0f 02 01 00

- No.: 166
- Timestamp: 20:28:25:564_0
- RFN: 128
- Chip: 16384
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Config_CNF
- Source: ts_SS_PCH_FACH_CCCH_Cfg LINE 6
- Message Structure:
CPHY_TrCH_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 5
- Constraint:
ca_TrChCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 05

- No.: 167
- Timestamp: 20:28:25:601_0
- RFN: 132
- Chip: 5376
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_SS_PCH_FACH_CCCH_Cfg LINE 7
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 5
. (RatType)ratType = 0
. configMessage
. . CmacConfigReq
. . . SS_ActivationTime
. . . UE_Info
. . . . U_RNTI
. . . . (BitStringType)c_RNTI[16] = -
. . . TrCHInfo
. . . . ulconnectedTrCHList
. . . . TFCS
. . . . dlconnectedTrCHList
. . . . . TrCHInfo_setseq_1
. . . . . . (IntegerType)trchid = 12
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 240
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional = 0
. . . . . . . . (IntegerType)rateMatchingAttribute = 230
. . . . . . . . (CRC_Size)crc_Size = 3
. . . . . TrCHInfo_setseq_1
. . . . . . (IntegerType)trchid = 13
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 168
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . (IntegerType)small = 2
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional = 0
. . . . . . . . (IntegerType)rateMatchingAttribute = 220
. . . . . . . . (CRC_Size)crc_Size = 3
. . . . . TrCHInfo_setseq_1
. . . . . . (IntegerType)trchid = 14
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 360
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . (IntegerType)rateMatchingAttribute = 130
. . . . . . . . (CRC_Size)crc_Size = 3
. . . . TFCS
. . . . . ExplicitTFCS_Configuration
. . . . . . TFCS_ReconfAdd
. . . . . . . ctfcSize
. . . . . . . . ctfc4Bit
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 0
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 1
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 2
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 3
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 4
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 5
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 6
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 8
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 11
. . . . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . TrCH_LogCHMappingList1
. . . . ulconnectedTrCHList
. . . . dlconnectedTrCHList
. . . . . TrCH_LogCHMappingList1_setseq_1
. . . . . . (IntegerType)trchid = 12
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 3
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 1
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 1
. . . . . . . . (IntegerType)rB_Identity = -2
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . TrCH_LogCHMappingList1_setseq_1
. . . . . . (IntegerType)trchid = 13
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 1
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 5
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 2
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 1
. . . . . . . . (IntegerType)rB_Identity = 0
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_CMAC_CfgInfo
- BinaryMessage:
30 82 01 23 02 01 00 02 01 05 0a 01 00 30 82 01 16 05 00 30 00 30 81 cd 30 6b 30 21 02 01 0c 30 1c 30 0e 30 0c 02 02 00 f0 30 04 05 00 05 00 05 00 30 0a 0a 01 00 02 02 00 e6 0a 01 03 30 24 02 01 0d 30 1f 30 11 30 0f 02 02 00 a8 30 07 05 00 05 00 02 01 02 05 00 30 0a 0a 01 00 02 02 00 dc 0a 01 03 30 20 02 01 0e 30 1b 30 0e 30 0c 02 02 01 68 30 04 05 00 05 00 05 00 30 09 05 00 02 02 00 82 0a 01 03 30 5e 30 30 5b 30 08 02 01 00 30 03 02 01 00 30 08 02 01 01 30 03 02 01 00 30 08 02 01 02 30 03 02 01 00 30 08 02 01 03 30 03 02 01 00 30 08 02 01 04 30 03 02 01 00 30 08 02 01 05 30 03 02 01 00 30 08 02 01 06 30 03 02 01 00 30 13 02 01 08 30 0e 30 0c 30 30 03 02 01 0b 02 01 0f 02 01 00 30 40 30 3e 30 1d 02 01 0c 30 18 30 16 30 11 0a 01 00 0a 01 03 02 01 01 0a 01 01 05 00 02 01 01 02 01 fe 30 1d 02 01 0d 30 18 30 16 30 11 0a 01 00 0a 01 01 02 01 05 0a 01 02 05 00 02 01 01 02 01 00

- No.: 171
- Timestamp: 20:28:25:650_0
- RFN: 136
- Chip: 37888
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_SS_PCH_FACH_CCCH_Cfg LINE 8
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 5
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 05

- No.: 172
- Timestamp: 20:28:25:654_0
- RFN: 137
- Chip: 15360
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_PCH_FACH_CCCH_Cfg LINE 9
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 6
. (RatType)ratType = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . PICHInfo
. . . . PICH_Info
. . . . . fdd
. . . . . . (IntegerType)channelisationCode256 = 2
. . . . . . (PI_CountPerFrame)pi_CountPerFrame = 0
. . . . . . (BooleanType)sttd_Indicator = FALSE
. . . . (IntegerType)dl_TxPower = -5
- Constraint:
ca_PICH_Info
- BinaryMessage:
30 1c 02 01 00 02 01 06 0a 01 00 30 11 30 0f 30 30 09 02 01 02 0a 01 00 01 01 00 02 01 fb

- No.: 176
- Timestamp: 20:28:25:662_0
- RFN: 138
- Chip: 8960
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_PCH_FACH_CCCH_Cfg LINE 10
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 6
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 06

- No.: 184
- Timestamp: 20:28:25:668_0
- RFN: 138
- Chip: 31488
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_RACH_CCCH_Cfg LINE 3
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 7
. (RatType)ratType = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . AICHInfo
. . . . AICH_Info
. . . . . (IntegerType)channelisationCode256 = 3
. . . . . (BooleanType)sttd_Indicator = FALSE
. . . . . (AICH_TransmissionTiming)aich_TransmissionTiming = 0
. . . . (IntegerType)dl_TxPower = -5
- Constraint:
ca_AichInfo
- BinaryMessage:
30 1b 02 01 00 02 01 07 0a 01 00 30 10 30 0e 30 09 02 01 03 01 01 00 0a 01 00 02 01 fb

- No.: 188
- Timestamp: 20:28:25:675_0
- RFN: 139
- Chip: 21248
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_RACH_CCCH_Cfg LINE 4
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 7
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 07

- No.: 189
- Timestamp: 20:28:25:680_0
- RFN: 140
- Chip: 1280
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_RACH_CCCH_Cfg LINE 5
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 8
. (RatType)ratType = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . PRACHInfo
. . . . fdd_tdd
. . . . . fdd
. . . . . . (BitStringType)preambleSignature[16] = "0000000011111111"
. . . . . . (SF_PRACH)spreadingFactorForDataPart = 1
. . . . . . (IntegerType)preambleScramblingCode = 0
. . . . . . (PuncturingLimit)puncturingLimit = 15
. . . . . . (BitStringType)accessSlot[12] = "111111111111"
- Constraint:
ca_PRACH_Info
- BinaryMessage:
30 23 02 01 00 02 01 08 0a 01 00 30 18 30 16 30 30 13 03 03 00 00 ff 0a 01 01 02 01 00 0a 01 0f 03 03 04 ff f0

- No.: 193
- Timestamp: 20:28:25:691_0
- RFN: 141
- Chip: 3840
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_RACH_CCCH_Cfg LINE 6
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 8
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 08

- No.: 194
- Timestamp: 20:28:25:702_0
- RFN: 142
- Chip: 8448
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Config_REQ
- Source: ts_SS_RACH_CCCH_Cfg LINE 7
- Message Structure:
CPHY_TrCH_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 8
. (RatType)ratType = 0
. CphyTrchConfigReq
. . SS_ActivationTime
. . ulconnectedTrCHList
. . . CphyTrchConfigReq_setseq_0
. . . . (IntegerType)trchid = 15
. . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 1
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 168
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 360
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional = 0
. . . . . . (IntegerType)rateMatchingAttribute = 150
. . . . . . (CRC_Size)crc_Size = 3
. . TFCS
. . . ExplicitTFCS_Configuration
. . . . TFCS_ReconfAdd
. . . . . ctfcSize
. . . . . . ctfc2Bit
. . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . (IntegerType)ctfc2 = 0
. . . . . . . . PowerOffsetInformation
. . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . (IntegerType)ctfc2 = 1
. . . . . . . . PowerOffsetInformation
. . dlconnectedTrCHList
. . TFCS
- Constraint:
cab_RACH_InfoActNow
- BinaryMessage:
30 4e 02 01 00 02 01 08 0a 01 00 30 43 05 00 30 30 30 2e 02 01 0f 0a 01 01 30 26 30 18 30 0a 02 02 00 a8 30 02 05 00 05 00 30 0a 02 02 01 68 30 02 05 00 05 00 30 0a 0a 01 00 02 02 00 96 0a 01 03 30 0d 30 30 0a 30 03 02 01 00 30 03 02 01 01

- No.: 198
- Timestamp: 20:28:25:710_0
- RFN: 143
- Chip: 1792
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Config_CNF
- Source: ts_SS_RACH_CCCH_Cfg LINE 8
- Message Structure:
CPHY_TrCH_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 8
- Constraint:
ca_TrChCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 08

- No.: 199
- Timestamp: 20:28:25:729_0
- RFN: 144
- Chip: 34816
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_SS_RACH_CCCH_Cfg LINE 9
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 8
. (RatType)ratType = 0
. configMessage
. . CmacConfigReq
. . . SS_ActivationTime
. . . UE_Info
. . . . U_RNTI
. . . . (BitStringType)c_RNTI[16] = -
. . . TrCHInfo
. . . . ulconnectedTrCHList
. . . . . TrCHInfo_setseq_0
. . . . . . (IntegerType)trchid = 15
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 168
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 360
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional = 0
. . . . . . . . (IntegerType)rateMatchingAttribute = 150
. . . . . . . . (CRC_Size)crc_Size = 3
. . . . TFCS
. . . . . ExplicitTFCS_Configuration
. . . . . . TFCS_ReconfAdd
. . . . . . . ctfcSize
. . . . . . . . ctfc2Bit
. . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . (IntegerType)ctfc2 = 0
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . (IntegerType)ctfc2 = 1
. . . . . . . . . . PowerOffsetInformation
. . . . dlconnectedTrCHList
. . . . TFCS
. . . TrCH_LogCHMappingList1
. . . . ulconnectedTrCHList
. . . . . TrCH_LogCHMappingList1_setseq_0
. . . . . . (IntegerType)trchid = 15
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 1
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 5
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 2
. . . . . . . . (IntegerType)rB_Identity = 0
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . dlconnectedTrCHList
- Constraint:
ca_CMAC_CfgInfo
- BinaryMessage:
30 6d 02 01 00 02 01 08 0a 01 00 30 62 05 00 30 00 30 3e 30 2d 30 2b 02 01 0f 30 26 30 18 30 0a 02 02 00 a8 30 02 05 00 05 00 30 0a 02 02 01 68 30 02 05 00 05 00 30 0a 0a 01 00 02 02 00 96 0a 01 03 30 0d 30 30 0a 30 03 02 01 00 30 03 02 01 01 30 1c 30 1a 30 18 02 01 0f 30 13 30 11 30 0c 0a 01 00 0a 01 01 02 01 05 0a 01 02 02 01 00

- No.: 203
- Timestamp: 20:28:25:735_0
- RFN: 145
- Chip: 22784
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_SS_RACH_CCCH_Cfg LINE 10
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 8
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 08

- No.: 240
- Timestamp: 20:28:25:755_0
- RFN: 147
- Chip: 21248
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_1DCH_DCCH_Cfg LINE 4
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
. (RatType)ratType = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . DPCHInfo
. . . . UL_DPCH_Info
. . . . DL_DPCHInfo
. . . . . DL_CommonInformation
. . . . . . DL_DPCH_InfoCommon
. . . . . . . cfnHandling
. . . . . . . . initialise
. . . . . . . . . (IntegerType)cfntargetsfnframeoffset = -
. . . . . . . modeSpecificInfo
. . . . . . . . fdd
. . . . . . . . . DL_DPCH_PowerControlInfo
. . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . fdd
. . . . . . . . . . . . (DPC_Mode)dpc_Mode = 0
. . . . . . . . . (IntegerType)powerOffsetPilot_pdpdch = 0
. . . . . . . . . Dl_rate_matching_restriction
. . . . . . . . . SF512_AndPilot
. . . . . . . . . . (PilotBits128)sfd128 = 0
. . . . . . . . . (PositionFixedOrFlexible)positionFixedOrFlexible = 0
. . . . . . . . . (BooleanType)tfci_Existence = FALSE
. . . . . . modeSpecificInfo
. . . . . . . fdd
. . . . . . . . (IntegerType)defaultDPCH_OffsetValue = 0
. . . . . . . . DPCH_CompressedModeInfo
. . . . . . . . (TX_DiversityMode)tx_DiversityMode = 0
. . . . . . . . SSDT_Information
. . . . . DL_DPCH_InfoPerRL
. . . . . . fdd
. . . . . . . (PCPICH_UsageForChannelEst)pCPICH_UsageForChannelEst = 0
. . . . . . . (IntegerType)dpch_FrameOffset = 0
. . . . . . . SecondaryCPICH_Info
. . . . . . . DL_ChannelisationCodeList
. . . . . . . . DL_ChannelisationCode
. . . . . . . . . (IntegerType)secondaryScramblingCode = 1
. . . . . . . . . SF512_AndCodeNumber
. . . . . . . . . . (IntegerType)sf128 = 0
. . . . . . . . . (ScramblingCodeChange)scramblingCodeChange = -
. . . . . . . (IntegerType)tpc_CombinationIndex = 0
. . . . . . . (SSDT_CellIdentity)ssdt_CellIdentity = -
. . . . . . . (ClosedLoopTimingAdjMode)closedLoopTimingAdjMode = -
. . . . . (IntegerType)powerOffsetOfTFCI_PO1 = 0
. . . . . (IntegerType)powerOffsetOfTPC_PO2 = 0
. . . . . (IntegerType)powerOffsetOfPILOT_PO3 = 0
. . . . . (IntegerType)dl_TxPower = -5
. . . . . (IntegerType)dl_TxPowerMax = 15
. . . . . (IntegerType)dl_TxPowerMin = -35
- Constraint:
ca_DL_DPCH_Info
- BinaryMessage:
30 5e 02 01 00 02 01 1a 0a 01 00 30 53 30 51 30 4f 30 25 30 1a 30 30 00 30 30 14 30 06 30 30 03 0a 01 00 02 01 00 0a 01 00 0a 01 00 01 01 00 30 30 06 02 01 00 0a 01 00 30 30 13 0a 01 00 02 01 00 30 08 30 06 02 01 01 02 01 00 02 01 00 02 01 00 02 01 00 02 01 00 02 01 fb 02 01 0f 02 01 dd

- No.: 244
- Timestamp: 20:28:25:762_0
- RFN: 148
- Chip: 11264
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_1DCH_DCCH_Cfg LINE 5
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 1a

- No.: 245
- Timestamp: 20:28:25:775_0
- RFN: 149
- Chip: 20480
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Config_REQ
- Source: ts_SS_1DCH_DCCH_Cfg LINE 6
- Message Structure:
CPHY_TrCH_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
. (RatType)ratType = 0
. CphyTrchConfigReq
. . SS_ActivationTime
. . ulconnectedTrCHList
. . TFCS
. . dlconnectedTrCHList
. . . CphyTrchConfigReq_setseq_1
. . . . (IntegerType)trchid = 10
. . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 148
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional = 1
. . . . . . (IntegerType)rateMatchingAttribute = 192
. . . . . . (CRC_Size)crc_Size = 3
. . TFCS
. . . ExplicitTFCS_Configuration
. . . . TFCS_ReconfAdd
. . . . . ctfcSize
. . . . . . ctfc2Bit
. . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . (IntegerType)ctfc2 = 0
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . (IntegerType)ctfc2 = 1
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . fdd
. . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 11
. . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
- Constraint:
ca_DCH_148_TTI_10_DL_InfoActNow
- BinaryMessage:
30 59 02 01 00 02 01 1a 0a 01 00 30 4e 05 00 30 26 30 24 02 01 0a 0a 01 00 30 1c 30 0e 30 0c 02 02 00 94 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 c0 0a 01 03 30 22 30 30 1f 30 08 02 01 00 30 03 02 01 00 30 13 02 01 01 30 0e 30 0c 30 30 03 02 01 0b 02 01 0f 02 01 00

- No.: 249
- Timestamp: 20:28:25:789_0
- RFN: 150
- Chip: 31744
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Config_CNF
- Source: ts_SS_1DCH_DCCH_Cfg LINE 7
- Message Structure:
CPHY_TrCH_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
ca_TrChCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 1a

- No.: 250
- Timestamp: 20:28:25:822_0
- RFN: 154
- Chip: 7424
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_SS_1DCH_DCCH_Cfg LINE 8
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
. (RatType)ratType = 0
. configMessage
. . CmacConfigReq
. . . SS_ActivationTime
. . . UE_Info
. . . . U_RNTI
. . . . (BitStringType)c_RNTI[16] = -
. . . TrCHInfo
. . . . ulconnectedTrCHList
. . . . TFCS
. . . . dlconnectedTrCHList
. . . . . TrCHInfo_setseq_1
. . . . . . (IntegerType)trchid = 10
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 148
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . (IntegerType)rateMatchingAttribute = 192
. . . . . . . . (CRC_Size)crc_Size = 3
. . . . TFCS
. . . . . ExplicitTFCS_Configuration
. . . . . . TFCS_ReconfAdd
. . . . . . . ctfcSize
. . . . . . . . ctfc2Bit
. . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . (IntegerType)ctfc2 = 0
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . (IntegerType)ctfc2 = 1
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 11
. . . . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . TrCH_LogCHMappingList1
. . . . ulconnectedTrCHList
. . . . dlconnectedTrCHList
. . . . . TrCH_LogCHMappingList1_setseq_1
. . . . . . (IntegerType)trchid = 10
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 1
. . . . . . . . (IntegerType)rB_Identity = 1
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 2
. . . . . . . . (IntegerType)rB_Identity = 2
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 3
. . . . . . . . (IntegerType)rB_Identity = 3
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 4
. . . . . . . . (IntegerType)rB_Identity = 4
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_CMAC_CfgInfo
- BinaryMessage:
30 81 c6 02 01 ff 02 01 1a 0a 01 00 30 81 ba 05 00 30 00 30 49 30 23 30 21 02 01 0a 30 1c 30 0e 30 0c 02 02 00 94 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 c0 0a 01 03 30 22 30 30 1f 30 08 02 01 00 30 03 02 01 00 30 13 02 01 01 30 0e 30 0c 30 30 03 02 01 0b 02 01 0f 02 01 00 30 69 30 67 30 65 02 01 0a 30 60 30 16 30 11 0a 01 00 0a 01 00 02 01 01 0a 01 04 05 00 02 01 01 02 01 01 30 16 30 11 0a 01 00 0a 01 00 02 01 02 0a 01 04 05 00 02 01 02 02 01 02 30 16 30 11 0a 01 00 0a 01 00 02 01 03 0a 01 04 05 00 02 01 03 02 01 03 30 16 30 11 0a 01 00 0a 01 00 02 01 04 0a 01 04 05 00 02 01 04 02 01 04

- No.: 254
- Timestamp: 20:28:25:838_0
- RFN: 155
- Chip: 28672
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_SS_1DCH_DCCH_Cfg LINE 9
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 1a

- No.: 255
- Timestamp: 20:28:25:843_0
- RFN: 156
- Chip: 12032
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_1DCH_DCCH_Cfg LINE 10
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
. (RatType)ratType = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . DPCHInfo
. . . . UL_DPCH_Info
. . . . . UL_DPCH_PowerControlInfo
. . . . . . fdd
. . . . . . . (IntegerType)dpcch_PowerOffset = -40
. . . . . . . (IntegerType)pc_Preamble = 1
. . . . . . . (IntegerType)sRB_delay = 7
. . . . . . . PowerControlAlgorithm
. . . . . . . . (IntegerType)algorithm1 = 1
. . . . . modeSpecificInfo
. . . . . . fdd
. . . . . . . (ScramblingCodeType)scramblingCodeType = 1
. . . . . . . (IntegerType)scramblingCode = 0
. . . . . . . (IntegerType)numberOfDPDCH = -
. . . . . . . (SpreadingFactor)spreadingFactor = 4
. . . . . . . (BooleanType)tfci_Existence = TRUE
. . . . . . . (IntegerType)numberOfFBI_Bits = -
. . . . . . . (PuncturingLimit)puncturingLimit = 15
. . . . DL_DPCHInfo
- Constraint:
ca_UL_DPCH_Info
- BinaryMessage:
30 30 02 01 00 02 01 14 0a 01 00 30 25 30 23 30 21 30 30 0c 02 01 d8 02 01 01 02 01 07 02 01 01 30 30 0f 0a 01 01 02 01 00 0a 01 04 01 01 ff 0a 01 0f

- No.: 259
- Timestamp: 20:28:25:850_0
- RFN: 156
- Chip: 36864
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_1DCH_DCCH_Cfg LINE 11
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 260
- Timestamp: 20:28:25:859_0
- RFN: 157
- Chip: 33792
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Config_REQ
- Source: ts_SS_1DCH_DCCH_Cfg LINE 12
- Message Structure:
CPHY_TrCH_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
. (RatType)ratType = 0
. CphyTrchConfigReq
. . SS_ActivationTime
. . ulconnectedTrCHList
. . . CphyTrchConfigReq_setseq_0
. . . . (IntegerType)trchid = 5
. . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 148
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional = 1
. . . . . . (IntegerType)rateMatchingAttribute = 192
. . . . . . (CRC_Size)crc_Size = 3
. . TFCS
. . . ExplicitTFCS_Configuration
. . . . TFCS_ReconfAdd
. . . . . ctfcSize
. . . . . . ctfc2Bit
. . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . (IntegerType)ctfc2 = 0
. . . . . . . . PowerOffsetInformation
. . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . (IntegerType)ctfc2 = 1
. . . . . . . . PowerOffsetInformation
. . dlconnectedTrCHList
. . TFCS
- Constraint:
ca_DCH_148_TTI_10_UL_InfoActNow
- BinaryMessage:
30 44 02 01 00 02 01 14 0a 01 00 30 39 05 00 30 26 30 24 02 01 05 0a 01 00 30 1c 30 0e 30 0c 02 02 00 94 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 c0 0a 01 03 30 0d 30 30 0a 30 03 02 01 00 30 03 02 01 01

- No.: 264
- Timestamp: 20:28:25:872_0
- RFN: 159
- Chip: 7168
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Config_CNF
- Source: ts_SS_1DCH_DCCH_Cfg LINE 13
- Message Structure:
CPHY_TrCH_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_TrChCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 265
- Timestamp: 20:28:25:906_0
- RFN: 162
- Chip: 21760
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_SS_1DCH_DCCH_Cfg LINE 14
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
. (RatType)ratType = 0
. configMessage
. . CmacConfigReq
. . . SS_ActivationTime
. . . UE_Info
. . . . U_RNTI
. . . . (BitStringType)c_RNTI[16] = -
. . . TrCHInfo
. . . . ulconnectedTrCHList
. . . . . TrCHInfo_setseq_0
. . . . . . (IntegerType)trchid = 5
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 148
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . (IntegerType)rateMatchingAttribute = 192
. . . . . . . . (CRC_Size)crc_Size = 3
. . . . TFCS
. . . . . ExplicitTFCS_Configuration
. . . . . . TFCS_ReconfAdd
. . . . . . . ctfcSize
. . . . . . . . ctfc2Bit
. . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . (IntegerType)ctfc2 = 0
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . (IntegerType)ctfc2 = 1
. . . . . . . . . . PowerOffsetInformation
. . . . dlconnectedTrCHList
. . . . TFCS
. . . TrCH_LogCHMappingList1
. . . . ulconnectedTrCHList
. . . . . TrCH_LogCHMappingList1_setseq_0
. . . . . . (IntegerType)trchid = 5
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . (IntegerType)rB_Identity = 1
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . (IntegerType)rB_Identity = 2
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . (IntegerType)rB_Identity = 3
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . (IntegerType)rB_Identity = 4
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . dlconnectedTrCHList
- Constraint:
ca_CMAC_CfgInfo
- BinaryMessage:
30 81 9d 02 01 ff 02 01 14 0a 01 00 30 81 91 05 00 30 00 30 34 30 23 30 21 02 01 05 30 1c 30 0e 30 0c 02 02 00 94 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 c0 0a 01 03 30 0d 30 30 0a 30 03 02 01 00 30 03 02 01 01 30 55 30 53 30 51 02 01 05 30 4c 30 11 30 0c 0a 01 00 0a 01 00 02 01 01 0a 01 04 02 01 01 30 11 30 0c 0a 01 00 0a 01 00 02 01 02 0a 01 04 02 01 02 30 11 30 0c 0a 01 00 0a 01 00 02 01 03 0a 01 04 02 01 03 30 11 30 0c 0a 01 00 0a 01 00 02 01 04 0a 01 04 02 01 04

- No.: 269
- Timestamp: 20:28:25:926_0
- RFN: 164
- Chip: 22528
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_SS_1DCH_DCCH_Cfg LINE 15
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 14

- No.: 272
- Timestamp: 20:28:25:932_0
- RFN: 165
- Chip: 6912
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB_BCCH_BCH_Cfg LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 246
. . . . . UL_RLC_Mode
. . . . . . UL_TM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . (BooleanType)segmentationIndication = FALSE
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = -
. . . . (IntegerType)dLlogicalChannelIdentity = 1
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_BCCH_Info
- BinaryMessage:
30 1d 02 01 00 02 01 ff 0a 01 00 30 12 30 0b 30 09 02 02 00 f6 30 03 01 01 00 30 03 02 01 01

- No.: 276
- Timestamp: 20:28:25:939_0
- RFN: 165
- Chip: 34560
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB_BCCH_BCH_Cfg LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 279
- Timestamp: 20:28:25:944_0
- RFN: 166
- Chip: 16896
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB_PCCH_Cfg LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -2
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 240
. . . . . UL_RLC_Mode
. . . . . . UL_TM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . (BooleanType)segmentationIndication = FALSE
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = -
. . . . (IntegerType)dLlogicalChannelIdentity = 1
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_PCCH_Info
- BinaryMessage:
30 1d 02 01 00 02 01 fe 0a 01 00 30 12 30 0b 30 09 02 02 00 f0 30 03 01 01 00 30 03 02 01 01

- No.: 283
- Timestamp: 20:28:25:951_0
- RFN: 167
- Chip: 4352
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB_PCCH_Cfg LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 fe

- No.: 286
- Timestamp: 20:28:25:957_0
- RFN: 167
- Chip: 27392
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB0_Cfg LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 152
. . . . . UL_RLC_Mode
. . . . . . UL_UM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (NoExplicitDiscard)timerBasedNoExplicit = 9
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = -
. . . . (IntegerType)dLlogicalChannelIdentity = 5
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_UM_DL_Info
- BinaryMessage:
30 1d 02 01 00 02 01 00 0a 01 00 30 12 30 0b 30 09 02 02 00 98 30 03 0a 01 09 30 03 02 01 05

- No.: 290
- Timestamp: 20:28:25:962_0
- RFN: 168
- Chip: 8448
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB0_Cfg LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 00

- No.: 291
- Timestamp: 20:28:25:968_0
- RFN: 168
- Chip: 31232
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB0_Cfg LINE 3
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_TM_RLC_Mode
. . . . . . (BooleanType)segmentationIndication = TRUE
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 166
. . . . . UL_RLC_Mode
. . . . . . UL_TM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . (BooleanType)segmentationIndication = TRUE
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = 5
. . . . (IntegerType)dLlogicalChannelIdentity = -
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_TM_UL_Info
- BinaryMessage:
30 22 02 01 00 02 01 00 0a 01 00 30 17 30 10 30 03 01 01 ff 30 09 02 02 00 a6 30 03 01 01 ff 30 03 02 01 05

- No.: 295
- Timestamp: 20:28:25:978_0
- RFN: 169
- Chip: 30976
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB0_Cfg LINE 4
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 00

- No.: 298
- Timestamp: 20:28:25:985_0
- RFN: 170
- Chip: 20736
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 136
. . . . . UL_RLC_Mode
. . . . . . UL_UM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (NoExplicitDiscard)timerBasedNoExplicit = 9
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = 1
. . . . (IntegerType)dLlogicalChannelIdentity = 1
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_UM_Info
- BinaryMessage:
30 22 02 01 ff 02 01 01 0a 01 00 30 17 30 0d 05 00 30 09 02 02 00 88 30 03 0a 01 09 30 06 02 01 01 02 01 01

- No.: 302
- Timestamp: 20:28:25:992_0
- RFN: 171
- Chip: 10752
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 303
- Timestamp: 20:28:26:001_0
- RFN: 172
- Chip: 4352
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 3
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . (TimerEPC)timerEPC = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . (TimerRST)timerRST = 9
. . . . . . . (MaxRST)max_RST = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = 2
. . . . (IntegerType)dLlogicalChannelIdentity = 2
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 02 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 27 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 02 02 01 02

- No.: 307
- Timestamp: 20:28:26:021_0
- RFN: 174
- Chip: 7424
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 4
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 308
- Timestamp: 20:28:26:030_0
- RFN: 175
- Chip: 3072
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 5
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . (TimerEPC)timerEPC = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . (TimerRST)timerRST = 9
. . . . . . . (MaxRST)max_RST = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = 3
. . . . (IntegerType)dLlogicalChannelIdentity = 3
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 03 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 27 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 03 02 01 03

- No.: 312
- Timestamp: 20:28:26:051_0
- RFN: 177
- Chip: 4352
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 6
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 313
- Timestamp: 20:28:26:060_0
- RFN: 178
- Chip: 1024
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 7
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . (TimerEPC)timerEPC = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . (TimerRST)timerRST = 9
. . . . . . . (MaxRST)max_RST = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = 4
. . . . (IntegerType)dLlogicalChannelIdentity = 4
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 04 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 27 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 04 02 01 04

- No.: 317
- Timestamp: 20:28:26:081_0
- RFN: 180
- Chip: 6656
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 8
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 358
- Timestamp: 20:28:26:128_0
- RFN: 184
- Chip: 30464
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 27
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 1b

- No.: 363
- Timestamp: 20:28:26:133_0
- RFN: 185
- Chip: 10240
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendNoSegDefSchedul LINE 2
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 364
- Timestamp: 20:28:26:137_0
- RFN: 185
- Chip: 26368
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendNoSegDefSchedul LINE 3
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 08 02 01 00 02 01 ff 00 00

- No.: 372
- Timestamp: 20:28:26:148_0
- RFN: 186
- Chip: 28160
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 11
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 0b

- No.: 377
- Timestamp: 20:28:26:152_0
- RFN: 187
- Chip: 7424
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB1 LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 378
- Timestamp: 20:28:26:157_0
- RFN: 187
- Chip: 27648
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB1 LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 1
. . . . . . . (BitStringType)sib_Data_variable[-1] = "1100010000000000000001011000100000101000000010100001000111100000000101000000000000000000000011000111010000"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 2
. . . . . . . (BitStringType)sib_Data_variable[-1] = "10000000000000000001"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 1c 02 01 00 02 01 ff 00 0e 21 69 c4 00 05 88 28 0a 11 e0 14 00 00 0c 74 04 27 00 00 20

- No.: 391
- Timestamp: 20:28:26:167_0
- RFN: 188
- Chip: 26880
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 11
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 0b

- No.: 396
- Timestamp: 20:28:26:178_0
- RFN: 189
- Chip: 29952
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB2 LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 397
- Timestamp: 20:28:26:183_0
- RFN: 190
- Chip: 11520
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB2 LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 1
. . . . . . . (BitStringType)sib_Data_variable[-1] = "1100010000000000000001011000100000101000000010100001000111100000000101000000000000000000000011000111010000"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 2
. . . . . . . (BitStringType)sib_Data_variable[-1] = "10000000000000000001"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 1c 02 01 00 02 01 ff 00 0e 21 69 c4 00 05 88 28 0a 11 e0 14 00 00 0c 74 04 27 00 00 20

- No.: 409
- Timestamp: 20:28:26:193_0
- RFN: 191
- Chip: 11264
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 10
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 0a

- No.: 414
- Timestamp: 20:28:26:200_0
- RFN: 192
- Chip: 512
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB3 LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 415
- Timestamp: 20:28:26:205_0
- RFN: 192
- Chip: 19712
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB3 LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 7
. . . . . . . (BitStringType)sib_Data_variable[-1] = "101000101000000010000001"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 3
. . . . . . . (BitStringType)sib_Data_variable[-1] = "110000000000000000000000000000000100000011001100011000000000100100001000000100011111111111111111111111"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 1c 02 01 00 02 01 ff 00 0e 27 17 a2 80 81 1b 2e 00 00 00 02 06 63 00 48 40 8f ff ff e0

- No.: 427
- Timestamp: 20:28:26:215_0
- RFN: 193
- Chip: 18688
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 26
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 1a

- No.: 432
- Timestamp: 20:28:26:220_0
- RFN: 194
- Chip: 1024
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB4 LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 433
- Timestamp: 20:28:26:225_0
- RFN: 194
- Chip: 19968
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB4 LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 7
. . . . . . . (BitStringType)sib_Data_variable[-1] = "101000101000000010000001"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 4
. . . . . . . (BitStringType)sib_Data_variable[-1] = "1000000000000000000000000000000101100110001100000000010010000100000010001110111"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 19 02 01 00 02 01 ff 00 0e 27 17 a2 80 81 22 74 00 00 00 0b 31 80 24 20 47 70

- No.: 450
- Timestamp: 20:28:26:269_0
- RFN: 198
- Chip: 35840
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 23
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 17

- No.: 455
- Timestamp: 20:28:26:278_0
- RFN: 199
- Chip: 33280
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB5 LINE 41
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 456
- Timestamp: 20:28:26:282_0
- RFN: 200
- Chip: 10240
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB5 LINE 42
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 08 02 01 00 02 01 ff 00 00

- No.: 460
- Timestamp: 20:28:26:286_0
- RFN: 200
- Chip: 24832
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 19
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 13

- No.: 465
- Timestamp: 20:28:26:299_0
- RFN: 201
- Chip: 34816
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB5 LINE 44
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 466
- Timestamp: 20:28:26:303_0
- RFN: 202
- Chip: 14592
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB5 LINE 45
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . FirstSegment
. . . . . . (SIB_Type)sib_Type = 5
. . . . . . (IntegerType)seg_Count = 3
. . . . . . (BitStringType)sib_Data_fixed[222] = "001101010100010000111110000000001111111101000011111111111111110111010010000100001111000000101001000011000000101010100101010110000000000000001100110001011011010101111110001010111010000011111110100000111111101000001111111010"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 25 02 01 00 02 01 ff 00 02 52 35 44 3e 00 ff 43 ff fd d2 10 f0 29 0c 0a a5 58 00 0c c5 b5 7e 2b a0 fe 83 fa 0f e8

- No.: 470
- Timestamp: 20:28:26:308_0
- RFN: 202
- Chip: 30464
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 21
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 15

- No.: 475
- Timestamp: 20:28:26:319_0
- RFN: 203
- Chip: 34816
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB5 LINE 47
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 476
- Timestamp: 20:28:26:323_0
- RFN: 204
- Chip: 14592
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB5 LINE 48
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . SubsequentSegment
. . . . . . (SIB_Type)sib_Type = 5
. . . . . . (IntegerType)segmentIndex = 1
. . . . . . (BitStringType)sib_Data_fixed[222] = "000011111111010000000000000000001101011000110100010000111111010011100101000001100001000011001010000000110000001110001001000000010110000000000000100000001110000000001000100001100100001010011001000010100000000000110000000100"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 25 02 01 00 02 01 ff 00 04 50 0f f4 00 00 d6 34 43 f4 e5 06 10 ca 03 03 89 01 60 00 80 e0 08 86 42 99 0a 00 30 10

- No.: 480
- Timestamp: 20:28:26:327_0
- RFN: 204
- Chip: 29952
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 22
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 16

- No.: 485
- Timestamp: 20:28:26:338_0
- RFN: 205
- Chip: 34304
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB5 LINE 50
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 487
- Timestamp: 20:28:26:343_0
- RFN: 206
- Chip: 14848
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB5 LINE 52
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . LastSegmentShort
. . . . . . (SIB_Type)sib_Type = 5
. . . . . . (IntegerType)segmentIndex = 2
. . . . . . (BitStringType)sib_Data_variable[-1] = "010001011100101011010110100000000000011110001000011000000001011011011011011000100000000001000011000010001001010000001011011010000000010000"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 1c 02 01 00 02 01 ff 00 06 51 89 45 ca d6 80 07 88 60 16 db 62 00 43 08 94 0b 68 04 00

- No.: 504
- Timestamp: 20:28:26:354_0
- RFN: 207
- Chip: 18176
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 3
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 03

- No.: 509
- Timestamp: 20:28:26:359_0
- RFN: 207
- Chip: 38144
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB6 LINE 8
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 512
- Timestamp: 20:28:26:364_0
- RFN: 208
- Chip: 18944
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB6:lt_CompleteSIB LINE 4
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 6
. . . . . . . (BitStringType)sib_Data_variable[-1] = "0000001010010001"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 0c 02 01 00 02 01 ff 00 0e 06 0f 02 91

- No.: 517
- Timestamp: 20:28:26:369_0
- RFN: 208
- Chip: 36096
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 5
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 05

- No.: 522
- Timestamp: 20:28:26:378_0
- RFN: 209
- Chip: 34304
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB6 LINE 11
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 523
- Timestamp: 20:28:26:382_0
- RFN: 210
- Chip: 11008
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB6 LINE 12
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 08 02 01 00 02 01 ff 00 00

- No.: 527
- Timestamp: 20:28:26:386_0
- RFN: 210
- Chip: 25088
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 6
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 06

- No.: 532
- Timestamp: 20:28:26:398_0
- RFN: 211
- Chip: 34560
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB6 LINE 14
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 533
- Timestamp: 20:28:26:402_0
- RFN: 212
- Chip: 11264
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB6 LINE 15
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 08 02 01 00 02 01 ff 00 00

- No.: 537
- Timestamp: 20:28:26:407_0
- RFN: 212
- Chip: 26368
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 7
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 07

- No.: 542
- Timestamp: 20:28:26:419_0
- RFN: 213
- Chip: 34304
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB6 LINE 17
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 543
- Timestamp: 20:28:26:423_0
- RFN: 214
- Chip: 11776
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB6 LINE 18
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 08 02 01 00 02 01 ff 00 00

- No.: 551
- Timestamp: 20:28:26:437_0
- RFN: 215
- Chip: 25344
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 2
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 02

- No.: 556
- Timestamp: 20:28:26:444_0
- RFN: 216
- Chip: 15104
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB7 LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 559
- Timestamp: 20:28:26:452_0
- RFN: 217
- Chip: 6912
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB7:lt_CompleteSIB LINE 4
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 7
. . . . . . . (BitStringType)sib_Data_variable[-1] = "101000101000000010000001"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 0d 02 01 00 02 01 ff 00 0e 07 17 a2 80 81

- No.: 567
- Timestamp: 20:28:26:467_0
- RFN: 218
- Chip: 25856
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 10
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 0a

- No.: 572
- Timestamp: 20:28:26:474_0
- RFN: 219
- Chip: 16640
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB7:lt_ConcatWithSIB3 LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 573
- Timestamp: 20:28:26:481_0
- RFN: 220
- Chip: 3840
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB7:lt_ConcatWithSIB3 LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 7
. . . . . . . (BitStringType)sib_Data_variable[-1] = "101000101000000010000001"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 3
. . . . . . . (BitStringType)sib_Data_variable[-1] = "110000000000000000000000000000000100000011001100011000000000100100001000000100011111111111111111111111"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 1c 02 01 00 02 01 ff 00 0e 27 17 a2 80 81 1b 2e 00 00 00 02 06 63 00 48 40 8f ff ff e0

- No.: 581
- Timestamp: 20:28:26:495_0
- RFN: 221
- Chip: 20224
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 18
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 12

- No.: 586
- Timestamp: 20:28:26:503_0
- RFN: 222
- Chip: 9984
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB7:lt_ConcatWithSIB18 LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 587
- Timestamp: 20:28:26:509_0
- RFN: 222
- Chip: 34560
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB7:lt_ConcatWithSIB18 LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 7
. . . . . . . (BitStringType)sib_Data_variable[-1] = "101000101000000010000001"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 26
. . . . . . . (BitStringType)sib_Data_variable[-1] = "100100000001000000000001000000001"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 13 02 01 00 02 01 ff 00 0e 27 17 a2 80 81 d1 04 80 80 08 04

- No.: 595
- Timestamp: 20:28:26:523_0
- RFN: 224
- Chip: 11520
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 26
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 1a

- No.: 600
- Timestamp: 20:28:26:530_0
- RFN: 225
- Chip: 768
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB7:lt_ConcatWithSIB4 LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 601
- Timestamp: 20:28:26:537_0
- RFN: 225
- Chip: 25856
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB7:lt_ConcatWithSIB4 LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 7
. . . . . . . (BitStringType)sib_Data_variable[-1] = "101000101000000010000001"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 4
. . . . . . . (BitStringType)sib_Data_variable[-1] = "1000000000000000000000000000000101100110001100000000010010000100000010001110111"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 19 02 01 00 02 01 ff 00 0e 27 17 a2 80 81 22 74 00 00 00 0b 31 80 24 20 47 70

- No.: 615
- Timestamp: 20:28:26:548_0
- RFN: 226
- Chip: 29440
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 31
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 1f

- No.: 620
- Timestamp: 20:28:26:558_0
- RFN: 227
- Chip: 32000
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB11 LINE 20
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 621
- Timestamp: 20:28:26:562_0
- RFN: 228
- Chip: 8704
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB11 LINE 21
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 08 02 01 00 02 01 ff 00 00

- No.: 625
- Timestamp: 20:28:26:566_0
- RFN: 228
- Chip: 23296
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 29
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 1d

- No.: 630
- Timestamp: 20:28:26:579_0
- RFN: 229
- Chip: 34560
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB11 LINE 23
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 631
- Timestamp: 20:28:26:584_0
- RFN: 230
- Chip: 14848
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB11 LINE 24
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . FirstSegment
. . . . . . (SIB_Type)sib_Type = 11
. . . . . . (IntegerType)seg_Count = 2
. . . . . . (BitStringType)sib_Data_fixed[222] = "011000001101100100010010000000001000110010000100001000010010010110101000100000100110010001010011000001011001000010100111000010111000010100001000100010001100100101010100000001001010000101001010100001100001001010001000001010"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 25 02 01 00 02 01 ff 00 02 b1 60 d9 12 00 8c 84 21 25 a8 82 64 53 05 90 a7 0b 85 08 88 c9 54 04 a1 4a 86 12 88 28

- No.: 635
- Timestamp: 20:28:26:588_0
- RFN: 230
- Chip: 32256
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 30
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 1e

- No.: 640
- Timestamp: 20:28:26:599_0
- RFN: 231
- Chip: 35072
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB11 LINE 26
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 642
- Timestamp: 20:28:26:604_0
- RFN: 232
- Chip: 15360
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB11 LINE 28
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . LastSegmentShort
. . . . . . (SIB_Type)sib_Type = 11
. . . . . . (IntegerType)segmentIndex = 1
. . . . . . (BitStringType)sib_Data_variable[-1] = "000100001100001001010010011010101000011000010010101000101100011001010100101010100001001111101000100010000001010010110000100010100001010101111000"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 1c 02 01 00 02 01 ff 00 06 b0 8f 10 c2 52 6a 86 12 a2 c6 54 aa 13 e8 88 14 b0 8a 15 78

- No.: 655
- Timestamp: 20:28:26:613_0
- RFN: 233
- Chip: 12032
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 13
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 0d

- No.: 660
- Timestamp: 20:28:26:620_0
- RFN: 234
- Chip: 768
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB12 LINE 8
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 663
- Timestamp: 20:28:26:625_0
- RFN: 234
- Chip: 21504
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB12:lt_CompleteSIB LINE 4
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 12
. . . . . . . (BitStringType)sib_Data_variable[-1] = "010000000"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 0c 02 01 00 02 01 ff 00 0e 0c 08 40 00

- No.: 668
- Timestamp: 20:28:26:629_0
- RFN: 234
- Chip: 37888
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 14
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 0e

- No.: 673
- Timestamp: 20:28:26:639_0
- RFN: 235
- Chip: 37120
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB12 LINE 11
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 674
- Timestamp: 20:28:26:643_0
- RFN: 236
- Chip: 13824
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB12 LINE 12
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 08 02 01 00 02 01 ff 00 00

- No.: 678
- Timestamp: 20:28:26:647_0
- RFN: 236
- Chip: 28672
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 15
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 0f

- No.: 683
- Timestamp: 20:28:26:658_0
- RFN: 237
- Chip: 34304
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB12 LINE 14
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 684
- Timestamp: 20:28:26:662_0
- RFN: 238
- Chip: 11008
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB12 LINE 15
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 08 02 01 00 02 01 ff 00 00

- No.: 692
- Timestamp: 20:28:26:670_0
- RFN: 239
- Chip: 3328
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 18
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 12

- No.: 697
- Timestamp: 20:28:26:680_0
- RFN: 240
- Chip: 1024
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB18 LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 698
- Timestamp: 20:28:26:685_0
- RFN: 240
- Chip: 20480
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB18 LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 7
. . . . . . . (BitStringType)sib_Data_variable[-1] = "101000101000000010000001"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 26
. . . . . . . (BitStringType)sib_Data_variable[-1] = "100100000001000000000001000000001"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 13 02 01 00 02 01 ff 00 0e 27 17 a2 80 81 d1 04 80 80 08 04

- No.: 710
- Timestamp: 20:28:26:694_0
- RFN: 241
- Chip: 16384
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 4
. . (IntegerType)sg_POS = 1
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 04 02 01 01

- No.: 715
- Timestamp: 20:28:26:700_0
- RFN: 242
- Chip: 768
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSB1_DefSchedul LINE 4
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 718
- Timestamp: 20:28:26:705_0
- RFN: 242
- Chip: 21504
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSB1_DefSchedul:lt_CompleteSIB LINE 4
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 27
. . . . . . . (BitStringType)sib_Data_variable[-1] = "10010000101010001000001100110000010010010100111000101001110100000000010110100010001101110010100010010010"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 17 02 01 00 02 01 ff 00 0e 1b 67 90 a8 83 30 49 4e 29 d0 05 a2 37 28 92

- No.: 736
- Timestamp: 20:28:26:716_0
- RFN: 243
- Chip: 25856
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 3
. . (IntegerType)sg_POS = 0
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 03 02 01 00

- No.: 741
- Timestamp: 20:28:26:722_0
- RFN: 244
- Chip: 5632
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendMIB LINE 7
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 744
- Timestamp: 20:28:26:727_0
- RFN: 244
- Chip: 27392
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendMIB:lt_CompleteSIB LINE 4
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 0
. . . . . . . (BitStringType)sib_Data_variable[-1] = "0001000000000000010000000010010110101010000100010000000000001000100010110000101000100010110001001000100010100001101000100110100010001110010010010011000100010000"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 1e 02 01 00 02 01 ff 00 0e 00 9f 10 00 40 25 aa 11 00 08 8b 0a 22 c4 88 a1 a2 68 8e 49 31 10

- No.: 759
- Timestamp: 20:28:26:734_0
- RFN: 245
- Chip: 13568
- Event: Send
- PCO: Ut
- Message: MMI_CmdReq
- Source: ts_MMI_UE_SwitchOn LINE 1
- Message Structure:
MMI_CmdReq
. (IA5StringType)cmd[-1] = "Please switch on the UE"
- Constraint:
ca_MMI_CmdReq
- BinaryMessage:
50 6c 65 61 73 65 20 73 77 69 74 63 68 20 6f 6e 20 74 68 65 20 55 45

- No.: 766
- Timestamp: 20:28:35:041_0
- RFN: 1076
- Chip: 3584
- Event: Receive
- PCO: Ut
- Message: MMI_CmdCnf
- Source: ts_MMI_UE_SwitchOn LINE 2
- Message Structure:
MMI_CmdCnf
. (BooleanType)result = TRUE
. (IA5StringType)resultString[6] = " OK "
- Constraint:
ca_MMI_CmdCnf
- BinaryMessage:
80 0d 0a 4f 4b 0d 0a

- No.: 782
- Timestamp: 20:28:35:051_0
- RFN: 1077
- Chip: 3584
- Event: Receive
- PCO: TM
- Message: RLC_TR_DATA_IND
- Source: ts_RRC_ConnEst:lt_RcvConnReq LINE 2
- Message Structure:
RLC_TR_DATA_IND
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
. tM_message
. . UL_CCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode = 0
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . UL_CCCH_MessageType
. . . . RRCConnectionRequest
. . . . . InitialUE_Identity
. . . . . . TMSI_and_LAI_GSM_MAP
. . . . . . . (BitStringType)tmsi[32] = "00010010001101000101011001111000"
. . . . . . . LAI
. . . . . . . . PLMN_Identity
. . . . . . . . . MCC
. . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . (IntegerType)_elem = 1
. . . . . . . . . MNC
. . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . (IntegerType)_elem = 1
. . . . . . . . (BitStringType)lac[16] = '0000000000000001'B
. . . . . (EstablishmentCause)establishmentCause = 12
. . . . . (ProtocolErrorIndicator)protocolErrorIndicator = 0
. . . . . MeasuredResultsOnRACH
. . . . . . currentCell
. . . . . . . modeSpecificInfo
. . . . . . . . fdd
. . . . . . . . . measurementQuantity
. . . . . . . . . . (IntegerType)cpich_Ec_N0 = 0
. . . . . v3d0NonCriticalExtensions
. . . . . . RRCConnectionRequest_v3d0ext_IEs
. . . . . . . (BitStringType)uESpecificBehaviourInformation1idle = 0
. . . . . . nonCriticalExtensions
- Constraint:
car_RRC_ConnReq
- BinaryMessage:
30 11 02 01 00 02 01 00 21 12 34 56 78 00 10 08 00 0b 00

- No.: 786
- Timestamp: 20:28:35:112_0
- RFN: 1083
- Chip: 9472
- Event: Send
- PCO: UM
- Message: RLC_UM_DATA_REQ
- Source: ts_RRC_ConnEst:lt_Send_ConnSetUp LINE 22
- Message Structure:
RLC_UM_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
. uM_message
. . DL_CCCH_Message
. . . IntegrityCheckInfo
. . . DL_CCCH_MessageType
. . . . RRCConnectionSetup
. . . . . r3
. . . . . . RRCConnectionSetup_r3_IEs
. . . . . . . InitialUE_Identity
. . . . . . . . TMSI_and_LAI_GSM_MAP
. . . . . . . . . (BitStringType)tmsi[32] = "00010010001101000101011001111000"
. . . . . . . . . LAI
. . . . . . . . . . PLMN_Identity
. . . . . . . . . . . MCC
. . . . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . . . (IntegerType)_elem = 1
. . . . . . . . . . . MNC
. . . . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . . . (IntegerType)_elem = 1
. . . . . . . . . . (BitStringType)lac[16] = '0000000000000001'B
. . . . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . . . (IntegerType)activationTime = -
. . . . . . . U_RNTI
. . . . . . . . (BitStringType)srnc_Identity[12] = "000000000001"
. . . . . . . . (BitStringType)s_RNTI[20] = "00000000000000000001"
. . . . . . . (BitStringType)new_c_RNTI[16] = -
. . . . . . . (RRC_StateIndicator)rrc_StateIndicator = 0
. . . . . . . (IntegerType)utran_DRX_CycleLengthCoeff = 9
. . . . . . . CapabilityUpdateRequirement
. . . . . . . . (BooleanType)ue_RadioCapabilityFDDUpdateRequirement = TRUE
. . . . . . . . (BooleanType)ue_RadioCapabilityTDDUpdateRequirement = FALSE
. . . . . . . . SystemSpecificCapUpdateReqList
. . . . . . . . . (SystemSpecificCapUpdateReq)_elem = 0
. . . . . . . SRB_InformationSetupList2
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_UM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 1
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 1
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . . . . . . . (TimerRST)timerRST = 9
. . . . . . . . . . . . . (MaxRST)max_RST = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 2
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 2
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . . . . . . . (TimerRST)timerRST = 9
. . . . . . . . . . . . . (MaxRST)max_RST = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 3
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 3
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . . . . . . . (TimerRST)timerRST = 9
. . . . . . . . . . . . . (MaxRST)max_RST = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 4
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 4
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . UL_CommonTransChInfo
. . . . . . . . TFC_Subset
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . TFCS
. . . . . . . . . . . ExplicitTFCS_Configuration
. . . . . . . . . . . . TFCS_ReconfAdd
. . . . . . . . . . . . . ctfcSize
. . . . . . . . . . . . . . ctfc2Bit
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . . . . . . . (IntegerType)ctfc2 = 0
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . . . . . . . (IntegerType)ctfc2 = 1
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 11
. . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . UL_AddReconfTransChInfoList
. . . . . . . . UL_AddReconfTransChInformation
. . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType = 0
. . . . . . . . . (IntegerType)transportChannelIdentity = 5
. . . . . . . . . TransportFormatSet
. . . . . . . . . . DedicatedTransChTFS
. . . . . . . . . . . tti
. . . . . . . . . . . . DedicatedDynamicTF_InfoList
. . . . . . . . . . . . . DedicatedDynamicTF_Info
. . . . . . . . . . . . . . rlc_Size
. . . . . . . . . . . . . . . BitModeRLC_SizeInfo
. . . . . . . . . . . . . . . . sizeType2
. . . . . . . . . . . . . . . . . (IntegerType)part1 = 2
. . . . . . . . . . . . . . . . . (IntegerType)part2 = -
. . . . . . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . LogicalChannelList
. . . . . . . . . . . SemistaticTF_Information
. . . . . . . . . . . . ChannelCodingType
. . . . . . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . . . . . (IntegerType)rateMatchingAttribute = 192
. . . . . . . . . . . . (CRC_Size)crc_Size = 3
. . . . . . . DL_CommonTransChInfo
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . dl_Parameters
. . . . . . . DL_AddReconfTransChInfoList
. . . . . . . . DL_AddReconfTransChInformation
. . . . . . . . . (DL_TrCH_Type)dl_TransportChannelType = 0
. . . . . . . . . (IntegerType)dl_transportChannelIdentity = 10
. . . . . . . . . tfs_SignallingMode
. . . . . . . . . . UL_TransportChannelIdentity
. . . . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType = 0
. . . . . . . . . . . (IntegerType)ul_TransportChannelIdentity = 5
. . . . . . . . . QualityTarget
. . . . . . . . . . (IntegerType)bler_QualityValue = -20
. . . . . . . . . TM_SignallingInfo
. . . . . . . FrequencyInfo
. . . . . . . (IntegerType)maxAllowedUL_TX_Power = -
. . . . . . . UL_ChannelRequirement
. . . . . . . . UL_DPCH_Info
. . . . . . . . . UL_DPCH_PowerControlInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (IntegerType)dpcch_PowerOffset = -40
. . . . . . . . . . . (IntegerType)pc_Preamble = 1
. . . . . . . . . . . (IntegerType)sRB_delay = 7
. . . . . . . . . . . PowerControlAlgorithm
. . . . . . . . . . . . (IntegerType)algorithm1 = 1
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (ScramblingCodeType)scramblingCodeType = 1
. . . . . . . . . . . (IntegerType)scramblingCode = 0
. . . . . . . . . . . (IntegerType)numberOfDPDCH = -
. . . . . . . . . . . (SpreadingFactor)spreadingFactor = 4
. . . . . . . . . . . (BooleanType)tfci_Existence = TRUE
. . . . . . . . . . . (IntegerType)numberOfFBI_Bits = -
. . . . . . . . . . . (PuncturingLimit)puncturingLimit = 15
. . . . . . . DL_CommonInformation
. . . . . . . . DL_DPCH_InfoCommon
. . . . . . . . . cfnHandling
. . . . . . . . . . initialise
. . . . . . . . . . . (IntegerType)cfntargetsfnframeoffset = -
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . DL_DPCH_PowerControlInfo
. . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . (DPC_Mode)dpc_Mode = 0
. . . . . . . . . . . (IntegerType)powerOffsetPilot_pdpdch = 0
. . . . . . . . . . . Dl_rate_matching_restriction
. . . . . . . . . . . SF512_AndPilot
. . . . . . . . . . . . (PilotBits128)sfd128 = 0
. . . . . . . . . . . (PositionFixedOrFlexible)positionFixedOrFlexible = 0
. . . . . . . . . . . (BooleanType)tfci_Existence = FALSE
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . (IntegerType)defaultDPCH_OffsetValue = 0
. . . . . . . . . . DPCH_CompressedModeInfo
. . . . . . . . . . (TX_DiversityMode)tx_DiversityMode = 0
. . . . . . . . . . SSDT_Information
. . . . . . . DL_InformationPerRL_List
. . . . . . . . DL_InformationPerRL
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . PrimaryCPICH_Info
. . . . . . . . . . . . (IntegerType)primaryScramblingCode = 100
. . . . . . . . . . . PDSCH_SHO_DCH_Info
. . . . . . . . . . . PDSCH_CodeMapping
. . . . . . . . . DL_DPCH_InfoPerRL
. . . . . . . . . . fdd
. . . . . . . . . . . (PCPICH_UsageForChannelEst)pCPICH_UsageForChannelEst = 0
. . . . . . . . . . . (IntegerType)dpch_FrameOffset = 0
. . . . . . . . . . . SecondaryCPICH_Info
. . . . . . . . . . . DL_ChannelisationCodeList
. . . . . . . . . . . . DL_ChannelisationCode
. . . . . . . . . . . . . (IntegerType)secondaryScramblingCode = 1
. . . . . . . . . . . . . SF512_AndCodeNumber
. . . . . . . . . . . . . . (IntegerType)sf128 = 0
. . . . . . . . . . . . . (ScramblingCodeChange)scramblingCodeChange = 1
. . . . . . . . . . . (IntegerType)tpc_CombinationIndex = 0
. . . . . . . . . . . (SSDT_CellIdentity)ssdt_CellIdentity = -
. . . . . . . . . . . (ClosedLoopTimingAdjMode)closedLoopTimingAdjMode = -
. . . . . . . . . SCCPCH_InfoForFACH
. . . . . . laterNonCriticalExtensions
. (BooleanType)specialLI = TRUE
- Constraint:
cas_RRC_ConnSetup
- BinaryMessage:
30 78 02 01 00 02 01 00 30 e7 22 46 8a cf 00 02 01 00 01 00 04 00 00 4d 82 69 3a 10 10 89 0d 42 00 02 81 9e 8e 46 c9 ce 7c 9c 4e 74 20 a5 12 3a 8c 00 15 13 3d 1c 8d 93 9c f9 38 9c e8 42 52 24 b5 28 00 4a 46 7a 39 1b 27 39 f2 71 39 d0 86 b4 49 ea 70 00 d4 c8 00 06 25 2b f0 02 00 08 82 23 bf 66 08 98 95 a5 47 a2 00 00 01 3f 90 0a 14 00 02 06 40 00 0c 28 08 01 01 ff

- No.: 807
- Timestamp: 20:28:35:156_1
- RFN: 1087
- Chip: 25088
- Event: Start Timer
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 3
- Message Structure:
no details available
- Constraint:
t_WaitMS (13500 Ms)
- BinaryMessage:

- No.: 812
- Timestamp: 20:28:35:378_0
- RFN: 1109
- Chip: 30976
- Event: Receive
- PCO: CPHY
- Message: CPHY_Sync_IND
- Source: RRC_Def1 LINE 13
- Message Structure:
CPHY_Sync_IND
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_SyncInd
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 813
- Timestamp: 20:28:35:378_1
- RFN: 1109
- Chip: 33024
- Event: Cancel Timer
- Source: RRC_Def1 LINE 13
- Message Structure:
no details available
- Constraint:
t_T312
- BinaryMessage:

- No.: 814
- Timestamp: 20:28:35:379_0
- RFN: 1109
- Chip: 35584
- Event: Default
- Source: RRC_Def1 LINE 0
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 815
- Timestamp: 20:28:35:379_1
- RFN: 1109
- Chip: 36608
- Event: Default
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 820
- Timestamp: 20:28:35:493_0
- RFN: 1121
- Chip: 12544
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_IND
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
RLC_AM_DATA_IND
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. IntegrityResult
. . (IntegrityStatus)integrityUsed = 0
. aM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode = 0
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . UL_DCCH_MessageType
. . . . RRCConnectionSetupComplete
. . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . STARTList
. . . . . . STARTSingle
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity = 1
. . . . . . . (BitStringType)start_Value[20] = "00000000000000000100"
. . . . . . STARTSingle
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity = 0
. . . . . . . (BitStringType)start_Value[20] = "00000000000000000010"
. . . . . UE_RadioAccessCapability
. . . . . . (AccessStratumReleaseIndicator)accessStratumReleaseIndicator = 0
. . . . . . PDCP_Capability
. . . . . . . (BooleanType)losslessSRNS_RelocationSupport = FALSE
. . . . . . . supportForRfc2507
. . . . . . RLC_Capability
. . . . . . . (TotalRLC_AM_BufferSize)totalRLC_AM_BufferSize = 2
. . . . . . . (MaximumRLC_WindowSize)maximumRLC_WindowSize = 0
. . . . . . . (MaximumAM_EntityNumberRLC_Cap)maximumAM_EntityNumber = 3
. . . . . . TransportChannelCapability
. . . . . . . DL_TransChCapability
. . . . . . . . (MaxNoBits)maxNoBitsReceived = 4
. . . . . . . . (MaxNoBits)maxConvCodeBitsReceived = 1
. . . . . . . . TurboSupport
. . . . . . . . . (MaxNoBits)supported = 4
. . . . . . . . (MaxSimultaneousTransChsDL)maxSimultaneousTransChs = 1
. . . . . . . . (IntegerType)maxSimultaneousCCTrCH_Count = 1
. . . . . . . . (MaxTransportBlocksDL)maxReceivedTransportBlocks = 2
. . . . . . . . (MaxNumberOfTFC_DL)maxNumberOfTFC = 4
. . . . . . . . (MaxNumberOfTF)maxNumberOfTF = 1
. . . . . . . UL_TransChCapability
. . . . . . . . (MaxNoBits)maxNoBitsTransmitted = 3
. . . . . . . . (MaxNoBits)maxConvCodeBitsTransmitted = 1
. . . . . . . . TurboSupport
. . . . . . . . . (MaxNoBits)supported = 3
. . . . . . . . (MaxSimultaneousTransChsUL)maxSimultaneousTransChs = 2
. . . . . . . . modeSpecificInfo
. . . . . . . . (MaxTransportBlocksUL)maxTransmittedBlocks = 2
. . . . . . . . (MaxNumberOfTFC_UL)maxNumberOfTFC = 3
. . . . . . . . (MaxNumberOfTF)maxNumberOfTF = 0
. . . . . . RF_Capability
. . . . . . . fddRF_Capability
. . . . . . . . (IntegerType)ue_PowerClass = 4
. . . . . . . . (TxRxFrequencySeparation)txRxFrequencySeparation = 0
. . . . . . . tddRF_Capability
. . . . . . . . (IntegerType)ue_PowerClass = 0
. . . . . . . . (RadioFrequencyBandTDDList)radioFrequencyTDDBandList = 0
. . . . . . . . (ChipRateCapability)chipRateCapability = 0
. . . . . . PhysicalChannelCapability
. . . . . . . fddPhysChCapability
. . . . . . . . DL_PhysChCapabilityFDD
. . . . . . . . . (IntegerType)maxNoDPCH_PDSCH_Codes = 3
. . . . . . . . . (MaxNoPhysChBitsReceived)maxNoPhysChBitsReceived = 6
. . . . . . . . . (BooleanType)supportForSF_512 = FALSE
. . . . . . . . . (BooleanType)supportOfPDSCH = FALSE
. . . . . . . . . SimultaneousSCCPCH_DPCH_Reception
. . . . . . . . UL_PhysChCapabilityFDD
. . . . . . . . . (MaxNoDPDCH_BitsTransmitted)maxNoDPDCH_BitsTransmitted = 2
. . . . . . . . . (BooleanType)supportOfPCPCH = FALSE
. . . . . . . tddPhysChCapability
. . . . . . . . DL_PhysChCapabilityTDD
. . . . . . . . . (IntegerType)maxTS_PerFrame = 0
. . . . . . . . . (IntegerType)maxPhysChPerFrame = 0
. . . . . . . . . (MinimumSF_DL)minimumSF = 0
. . . . . . . . . (BooleanType)supportOfPDSCH = FALSE
. . . . . . . . . (IntegerType)maxPhysChPerTS = 0
. . . . . . . . UL_PhysChCapabilityTDD
. . . . . . . . . (IntegerType)maxTS_PerFrame = 0
. . . . . . . . . (MaxPhysChPerTimeslot)maxPhysChPerTimeslot = 0
. . . . . . . . . (MinimumSF_UL)minimumSF = 0
. . . . . . . . . (BooleanType)supportOfPUSCH = FALSE
. . . . . . UE_MultiModeRAT_Capability
. . . . . . . MultiRAT_Capability
. . . . . . . . (BooleanType)supportOfGSM = TRUE
. . . . . . . . (BooleanType)supportOfMulticarrier = FALSE
. . . . . . . (MultiModeCapability)multiModeCapability = 1
. . . . . . SecurityCapability
. . . . . . . (BitStringType)cipheringAlgorithmCap[16] = '0000000000000011'B
. . . . . . . (BitStringType)integrityProtectionAlgorithmCap[16] = '0000000000000010'B
. . . . . . UE_Positioning_Capability
. . . . . . . (BooleanType)standaloneLocMethodsSupported = FALSE
. . . . . . . (BooleanType)ue_BasedOTDOA_Supported = FALSE
. . . . . . . (NetworkAssistedGPS_Supported)networkAssistedGPS_Supported = 3
. . . . . . . (BooleanType)supportForUE_GPS_TimingOfCellFrames = FALSE
. . . . . . . (BooleanType)supportForIPDL = FALSE
. . . . . . MeasurementCapability
. . . . . . . CompressedModeMeasCapability
. . . . . . . . (BooleanType)fdd_Measurements = TRUE
. . . . . . . . (BooleanType)tdd_Measurements = FALSE
. . . . . . . . GSM_Measurements
. . . . . . . . . (BooleanType)gsm900 = TRUE
. . . . . . . . . (BooleanType)dcs1800 = TRUE
. . . . . . . . . (BooleanType)gsm1900 = FALSE
. . . . . . . . (BooleanType)multiCarrierMeasurements = FALSE
. . . . . . . CompressedModeMeasCapability
. . . . . . . . (BooleanType)fdd_Measurements = TRUE
. . . . . . . . (BooleanType)tdd_Measurements = FALSE
. . . . . . . . GSM_Measurements
. . . . . . . . . (BooleanType)gsm900 = TRUE
. . . . . . . . . (BooleanType)dcs1800 = TRUE
. . . . . . . . . (BooleanType)gsm1900 = FALSE
. . . . . . . . (BooleanType)multiCarrierMeasurements = FALSE
. . . . . v370NonCriticalExtensions
. . . . . . RRCConnectionSetupComplete_v370ext
. . . . . . . UE_RadioAccessCapability_v370ext
. . . . . . v380NonCriticalExtensions
. . . . . . . RRCConnectionSetupComplete_v380ext_IEs
. . . . . . . . UE_RadioAccessCapability_v380ext
. . . . . . . . . UE_PositioningCapabilityExt_v380
. . . . . . . . . . (BooleanType)rx_tx_TimeDifferenceType2Capable = FALSE
. . . . . . . . DL_PhysChCapabilityFDD_v380ext
. . . . . . . . . (SupportOfDedicatedPilotsForChEstimation)supportOfDedicatedPilotsForChEstimation = 0
. . . . . . . v3a0NonCriticalExtensions
. . . . . . . . RRCConnectionSetupComplete_v3a0ext_IEs
. . . . . . . . . UE_RadioAccessCapability_v3a0ext
. . . . . . . . . . UE_PositioningCapabilityExt_v3a0
. . . . . . . . . . . (UE_PositioningCapabilityExt_v3a0_list_0)validity_CellPCH_UraPCH = 0
. . . . . . . . laterNonCriticalExtensions
. . . . . . . . . (BitStringType)rrcConnectionSetupComplete_r3_add_ext = 0
. . . . . . . . . nonCriticalExtensions
- Constraint:
car_RRC_ConnSetupCmpl
- BinaryMessage:
30 27 02 01 ff 02 01 02 0a 05 01 00 00 00 00 4a 0c 00 01 00 00 05 11 a0 d1 04 84 c6 68 46 2c 93 02 48 00 18 00 11 8f 8f 80

- No.: 821
- Timestamp: 20:28:35:504_0
- RFN: 1122
- Chip: 15104
- Event: Cancel Timer
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
t_WaitMS
- BinaryMessage:

- No.: 822
- Timestamp: 20:28:35:505_0
- RFN: 1122
- Chip: 16128
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 836
- Timestamp: 20:28:35:511_0
- RFN: 1123
- Chip: 2048
- Event: Send
- PCO: CMAC
- Message: CMAC_SecurityMode_Config_REQ
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 1
- Message Structure:
CMAC_SecurityMode_Config_REQ
. (IntegerType)cellId = 0
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity = 1
. . (BitStringType)startValue[20] = "00000000000000000100"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = -
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CMAC_SecurityModeCfgReq
- BinaryMessage:
30 0e 02 01 00 30 09 0a 01 01 03 04 04 00 00 40

- No.: 837
- Timestamp: 20:28:35:513_0
- RFN: 1123
- Chip: 8448
- Event: Receive
- PCO: CMAC
- Message: CMAC_SecurityMode_Config_CNF
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 2
- Message Structure:
CMAC_SecurityMode_Config_CNF
. (IntegerType)cellId = 0
- Constraint:
ca_CMAC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 00

- No.: 838
- Timestamp: 20:28:35:514_0
- RFN: 1123
- Chip: 15616
- Event: Send
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_REQ
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 3
- Message Structure:
CRLC_SecurityMode_Config_REQ
. (IntegerType)cellId = -1
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity = 1
. . (BitStringType)startValue[20] = "00000000000000000100"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = -
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CRLC_SecurityModeCfgReq
- BinaryMessage:
30 0e 02 01 ff 30 09 0a 01 01 03 04 04 00 00 40

- No.: 839
- Timestamp: 20:28:35:516_0
- RFN: 1123
- Chip: 21504
- Event: Receive
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_CNF
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 4
- Message Structure:
CRLC_SecurityMode_Config_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 853
- Timestamp: 20:28:35:521_0
- RFN: 1124
- Chip: 2816
- Event: Send
- PCO: CMAC
- Message: CMAC_SecurityMode_Config_REQ
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 1
- Message Structure:
CMAC_SecurityMode_Config_REQ
. (IntegerType)cellId = 0
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity = 0
. . (BitStringType)startValue[20] = "00000000000000000010"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = -
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CMAC_SecurityModeCfgReq
- BinaryMessage:
30 0e 02 01 00 30 09 0a 01 00 03 04 04 00 00 20

- No.: 854
- Timestamp: 20:28:35:523_0
- RFN: 1124
- Chip: 8960
- Event: Receive
- PCO: CMAC
- Message: CMAC_SecurityMode_Config_CNF
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 2
- Message Structure:
CMAC_SecurityMode_Config_CNF
. (IntegerType)cellId = 0
- Constraint:
ca_CMAC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 00

- No.: 855
- Timestamp: 20:28:35:524_0
- RFN: 1124
- Chip: 15872
- Event: Send
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_REQ
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 3
- Message Structure:
CRLC_SecurityMode_Config_REQ
. (IntegerType)cellId = -1
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity = 0
. . (BitStringType)startValue[20] = "00000000000000000010"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = -
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CRLC_SecurityModeCfgReq
- BinaryMessage:
30 0e 02 01 ff 30 09 0a 01 00 03 04 04 00 00 20

- No.: 856
- Timestamp: 20:28:35:526_0
- RFN: 1124
- Chip: 22272
- Event: Receive
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_CNF
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 4
- Message Structure:
CRLC_SecurityMode_Config_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 863
- Timestamp: 20:28:35:536_0
- RFN: 1125
- Chip: 22272
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_GMM_IdleUpdated:lt_IdleUpdated_NMO_II LINE 3
- Message Structure:
RRC_DataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain = 0
. (START_Value)start[20] = '00000000000000000010'B
. LOCATIONUPDATINGREQUEST
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)mMProtocolDiscriminator[4] = '0101'B
. . (MsgType)msgType[8] = '00001000'B
. . CiphKeySeqNum
. . . (B1)spare1[1] = '0'B
. . . (KeySeq)keySeq[3] = '000'B
. . LocUpdType
. . . (B1)fOR[1] = '0'B
. . . (B1)spare1[1] = '0'B
. . . (B2)lUT[2] = '10'B
. . LocAreaId_v
. . . (OctetStringType)plmn[3] = '00F110'O
. . . (OctetStringType)lac[2] = '0001'O
. . MS_Clsmk1
. . . (B1)spare1[1] = '0'B
. . . (B2)revLvl[2] = '10'B
. . . (B1)eSIND[1] = '0'B
. . . (B1)a5_1[1] = '1'B
. . . (B3)rFPwrCap[3] = '111'B
. . MS_Identity_lv
. . . (Length)iel[1] = '05'O
. . . (B4)iDigit1[4] = '1111'B
. . . (B1)oddEvenInd[1] = '0'B
. . . (B3)typeOfId[3] = '100'B
. . . (OctetStringType)otherDigits[4] = '12345678'O
. . MS_Clsmk2
. . . (IEI8)iei[8] = '00110011'B
. . . (Length)iel[1] = '03'O
. . . (B1)spare1_1[1] = '0'B
. . . (B2)revLvl[2] = '10'B
. . . (B1)eSIND[1] = '0'B
. . . (B1)a5_1[1] = '1'B
. . . (B3)rFPwrCap[3] = '111'B
. . . (B1)spare1_2[1] = '0'B
. . . (B1)pSCap[1] = '0'B
. . . (B2)sSSI[2] = '01'B
. . . (B1)sMCap[1] = '1'B
. . . (B1)vBS[1] = '0'B
. . . (B1)vGCS[1] = '0'B
. . . (B1)fC[1] = '0'B
. . . (B1)cM3[1] = '1'B
. . . (B1)spare1_3[1] = '0'B
. . . (B1)lCSVA[1] = '0'B
. . . (B1)uCS2[1] = '0'B
. . . (B1)soLSA[1] = '0'B
. . . (B1)cMSP[1] = '0'B
. . . (B1)a5_3[1] = '0'B
. . . (B1)a5_2[1] = '0'B
- Constraint:
car_InitDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 00 03 04 04 00 00 20 05 08 02 00 f1 10 00 01 4f 05 f4 12 34 56 78 33 03 4f 18 80

- No.: 900
- Timestamp: 20:28:35:558_0
- RFN: 1127
- Chip: 29440
- Event: Send
- PCO: Dc
- Message: RRC_DataReq
- Source: ts_MM_Authentication LINE 2
- Message Structure:
RRC_DataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[-1] = -
. (SapId)sapId[1] = -
. (SS_CN_DomainIdentity)cN_Domain = 0
. AUTHENTICATIONREQUEST
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)mMProtocolDiscriminator[4] = '0101'B
. . (MsgType)msgType[8] = '00010010'B
. . (B4)spare4[4] = '0000'B
. . CiphKeySeqNum
. . . (B1)spare1[1] = '0'B
. . . (KeySeq)keySeq[3] = '000'B
. . (MM_RAND)rAND[128] = '01010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101'B
. . AUTN
. . . (IEI8)iei[8] = '00100000'B
. . . (Length)iel[1] = '10'O
. . . (BitStringType)aUTN[128] = '01010110010100010101000001010011010100100101110100000000000000000101010101010100010101110101011001010001010100000101001101010010'B
- Constraint:
ca_DataReq
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 00 05 12 00 55 55 55 55 55 55 55 55 55 55 55 55 55 55 55 55 20 10 56 51 50 53 52 5d 00 00 55 54 57 56 51 50 53 52

- No.: 904
- Timestamp: 20:28:36:135_0
- RFN: 1185
- Chip: 17152
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_MM_Authentication LINE 7
- Message Structure:
RRC_DataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain = 0
. (START_Value)start[0] = -
. AUTHENTICATIONRESPONSE
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)mMProtocolDiscriminator[4] = '0101'B
. . (MsgType)msgType[8] = '01010100'B
. . (AuthRsp)authRsp[32] = '01010101010101000101011101010110'B
. . AuthRspExt
- Constraint:
car_UplinkDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 00 05 54 55 54 57 56

- No.: 942
- Timestamp: 20:28:36:149_0
- RFN: 1186
- Chip: 32256
- Event: Send
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_REQ
- Source: ts_SS_DownloadSecurityKey:lt_DownloadKeyCRLC LINE 1
- Message Structure:
CRLC_SecurityMode_Config_REQ
. (IntegerType)cellId = -1
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity = 0
. . (BitStringType)startValue[20] = "00000000000000000000"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = '01010111010101100101000101010000010100110101001001011101010111000101111101011110010110010101100001011011010110100101010101010100'B
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CRLC_SecurityModeCfgReq
- BinaryMessage:
30 21 02 01 ff 30 1c 0a 01 00 03 04 04 00 00 00 03 11 00 57 56 51 50 53 52 5d 5c 5f 5e 59 58 5b 5a 55 54

- No.: 943
- Timestamp: 20:28:36:150_0
- RFN: 1187
- Chip: 1280
- Event: Receive
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_CNF
- Source: ts_SS_DownloadSecurityKey:lt_DownloadKeyCRLC LINE 2
- Message Structure:
CRLC_SecurityMode_Config_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 950
- Timestamp: 20:28:36:154_0
- RFN: 1187
- Chip: 13824
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 1
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
. (IntegerType)count_I_LSB_UL = -
. (IntegerType)count_I_LSB_DL = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 00 02 01 00 02 01 00

- No.: 951
- Timestamp: 20:28:36:156_0
- RFN: 1187
- Chip: 20992
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 2
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 00 02 01 00

- No.: 952
- Timestamp: 20:28:36:158_0
- RFN: 1187
- Chip: 28416
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 3
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. (IntegerType)count_I_LSB_UL = -
. (IntegerType)count_I_LSB_DL = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 01 02 01 00

- No.: 953
- Timestamp: 20:28:36:159_0
- RFN: 1187
- Chip: 35328
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 4
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 954
- Timestamp: 20:28:36:161_0
- RFN: 1188
- Chip: 4096
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 5
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. (IntegerType)count_I_LSB_UL = -
. (IntegerType)count_I_LSB_DL = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 02 02 01 00

- No.: 955
- Timestamp: 20:28:36:163_0
- RFN: 1188
- Chip: 11520
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 6
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 956
- Timestamp: 20:28:36:165_0
- RFN: 1188
- Chip: 18432
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 7
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
. (IntegerType)count_I_LSB_UL = -
. (IntegerType)count_I_LSB_DL = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 03 02 01 00

- No.: 957
- Timestamp: 20:28:36:167_0
- RFN: 1188
- Chip: 25344
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 8
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 958
- Timestamp: 20:28:36:169_0
- RFN: 1188
- Chip: 32768
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 9
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
. (IntegerType)count_I_LSB_UL = -
. (IntegerType)count_I_LSB_DL = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 04 02 01 00

- No.: 959
- Timestamp: 20:28:36:171_0
- RFN: 1189
- Chip: 1536
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 10
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 963
- Timestamp: 20:28:36:174_0
- RFN: 1189
- Chip: 12800
- Event: Send
- PCO: CRLC
- Message: CRLC_Integrity_Activate_REQ
- Source: ts_CRLC_DL_Integrity LINE 1
- Message Structure:
CRLC_Integrity_Activate_REQ
. (IntegerType)cellId = -1
. (CN_DomainIdentity)cn_DomainIdentity = 0
. IntegrityActivationInfo
. . IntegrityProtectionModeInfo
. . . IntegrityProtectionModeCommand
. . . . startIntegrityProtection
. . . . . (BitStringType)integrityProtInitNumber[32] = "00000000000000000000000000000001"
. . . (IntegrityProtectionAlgorithm)integrityProtectionAlgorithm = 0
- Constraint:
ca_CRLC_DL_IntegrityActivateReq
- BinaryMessage:
30 15 02 01 ff 0a 01 00 30 0d 30 30 07 03 05 00 00 00 00 01 0a 01 00

- No.: 964
- Timestamp: 20:28:36:175_0
- RFN: 1189
- Chip: 19200
- Event: Receive
- PCO: CRLC
- Message: CRLC_Integrity_Activate_CNF
- Source: ts_CRLC_DL_Integrity LINE 2
- Message Structure:
CRLC_Integrity_Activate_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_IntegrityActivateCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 971
- Timestamp: 20:28:36:179_0
- RFN: 1189
- Chip: 33792
- Event: Send
- PCO: CRLC
- Message: CRLC_Integrity_Activate_REQ
- Source: ts_RB2_UL_IntegrityActivate LINE 1
- Message Structure:
CRLC_Integrity_Activate_REQ
. (IntegerType)cellId = -1
. (CN_DomainIdentity)cn_DomainIdentity = 0
. IntegrityActivationInfo
. . IntegrityProtActivationInfoList
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity = 2
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
- Constraint:
ca_CRLC_UL_IntegrityActivateReq
- BinaryMessage:
30 10 02 01 ff 0a 01 00 30 08 30 06 02 01 02 02 01 00

- No.: 972
- Timestamp: 20:28:36:181_0
- RFN: 1190
- Chip: 1536
- Event: Receive
- PCO: CRLC
- Message: CRLC_Integrity_Activate_CNF
- Source: ts_RB2_UL_IntegrityActivate LINE 2
- Message Structure:
CRLC_Integrity_Activate_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_IntegrityActivateCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 978
- Timestamp: 20:28:36:187_0
- RFN: 1190
- Chip: 25344
- Event: Send
- PCO: AM
- Message: RLC_AM_DATA_REQ
- Source: ts_RRC_Security:lt_SendSecurityModeCommand LINE 7
- Message Structure:
RLC_AM_DATA_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. AmConfirmationRequest
. aM_message
. . DL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00000000000000000000000000000000"
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . DL_DCCH_MessageType
. . . . SecurityModeCommand
. . . . . r3
. . . . . . SecurityModeCommand_r3_IEs
. . . . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . . . SecurityCapability
. . . . . . . . (BitStringType)cipheringAlgorithmCap[16] = '0000000000000011'B
. . . . . . . . (BitStringType)integrityProtectionAlgorithmCap[16] = '0000000000000010'B
. . . . . . . CipheringModeInfo
. . . . . . . IntegrityProtectionModeInfo
. . . . . . . . IntegrityProtectionModeCommand
. . . . . . . . . startIntegrityProtection
. . . . . . . . . . (BitStringType)integrityProtInitNumber[32] = "00000000000000000000000000000001"
. . . . . . . . (IntegrityProtectionAlgorithm)integrityProtectionAlgorithm = 0
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity = 0
. . . . . . . InterRAT_UE_SecurityCapList
. . . . . . laterNonCriticalExtensions
- Constraint:
cas_RRC_SecModeCmd
- BinaryMessage:
30 17 02 01 ff 02 01 02 05 00 80 00 00 00 04 04 00 01 80 01 40 00 00 00 20

- No.: 984
- Timestamp: 20:28:36:323_0
- RFN: 1204
- Chip: 12032
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_IND
- Source: ts_RRC_Security:lt_StartSecurity_UE LINE 8
- Message Structure:
RLC_AM_DATA_IND
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. IntegrityResult
. . (IntegrityStatus)integrityUsed = 0
. aM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "10000001100000001110110111011101"
. . . . (IntegerType)rrc_MessageSequenceNumber = 1
. . . UL_DCCH_MessageType
. . . . SecurityModeComplete
. . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . IntegrityProtActivationInfo
. . . . . . RRC_MessageSequenceNumberList
. . . . . . . (IntegerType)_elem = 0
. . . . . . . (IntegerType)_elem = 0
. . . . . . . (IntegerType)_elem = 0
. . . . . . . (IntegerType)_elem = 0
. . . . . . . (IntegerType)_elem = 0
. . . . . laterNonCriticalExtensions
. . . . . . (BitStringType)securityModeComplete_r3_add_ext = 0
. . . . . . nonCriticalExtensions
- Constraint:
car_RRC_SecModeCmpl
- BinaryMessage:
30 12 02 01 ff 02 01 02 0a 01 00 c0 c0 76 ee 8d 21 00 00 00

- No.: 985
- Timestamp: 20:28:36:324_0
- RFN: 1204
- Chip: 16384
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_Security:lt_StartSecurity_UE LINE 8
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 987
- Timestamp: 20:28:36:328_0
- RFN: 1204
- Chip: 31744
- Event: Send
- PCO: CRLC
- Message: CRLC_Integrity_Activate_REQ
- Source: ts_CRLC_UL_Integrity LINE 1
- Message Structure:
CRLC_Integrity_Activate_REQ
. (IntegerType)cellId = -1
. (CN_DomainIdentity)cn_DomainIdentity = 0
. IntegrityActivationInfo
. . IntegrityProtActivationInfoList
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity = 0
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity = 1
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity = 3
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity = 4
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
- Constraint:
ca_CRLC_UL_IntegrityActivateReq
- BinaryMessage:
30 28 02 01 ff 0a 01 00 30 20 30 06 02 01 00 02 01 00 30 06 02 01 01 02 01 00 30 06 02 01 03 02 01 00 30 06 02 01 04 02 01 00

- No.: 988
- Timestamp: 20:28:36:330_0
- RFN: 1205
- Chip: 768
- Event: Receive
- PCO: CRLC
- Message: CRLC_Integrity_Activate_CNF
- Source: ts_CRLC_UL_Integrity LINE 2
- Message Structure:
CRLC_Integrity_Activate_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_IntegrityActivateCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 995
- Timestamp: 20:28:36:335_0
- RFN: 1205
- Chip: 21504
- Event: Send
- PCO: Dc
- Message: RRC_DataReq
- Source: ts_GMM_IdleUpdated:lt_LocUpdAcc LINE 2
- Message Structure:
RRC_DataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[-1] = -
. (SapId)sapId[1] = -
. (SS_CN_DomainIdentity)cN_Domain = 0
. LOCATIONUPDATINGACCEPT
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)mMProtocolDiscriminator[4] = '0101'B
. . (MsgType)msgType[8] = '00000010'B
. . LocAreaId_v
. . . (OctetStringType)plmn[3] = '00F110'O
. . . (OctetStringType)lac[2] = '0001'O
. . MM_MS_Identity
. . . (IEI8)iei[8] = '00010111'B
. . . (Length)iel[1] = '05'O
. . . (B4)iDigit1[4] = '1111'B
. . . (B1)oddEvenInd[1] = '0'B
. . . (B3)typeOfId[3] = '100'B
. . . (OctetStringType)otherDigits[-1] = '12345678'O
. . (FollowOnProceed)followOnProceed[8] = '10100001'B
. . (CTSPerm)cTSPerm[8] = '10100010'B
. . PLMN_List
- Constraint:
ca_DataReq
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 00 05 02 00 f1 10 00 01 17 05 f4 12 34 56 78 a1 a2

- No.: 999
- Timestamp: 20:28:36:472_0
- RFN: 1219
- Chip: 5888
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_GMM_IdleUpdated:lt_LocUpdAcc LINE 3
- Message Structure:
RRC_DataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain = 0
. (START_Value)start[0] = -
. TMSIREALLOCATIONCOMPLETE
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)mMProtocolDiscriminator[4] = '0101'B
. . (MsgType)msgType[8] = '10011011'B
- Constraint:
car_UplinkDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 00 05 9b

- No.: 1013
- Timestamp: 20:28:36:476_2
- RFN: 1219
- Chip: 23552
- Event: Start Timer
- Source: ts_RRC_Delay LINE 1
- Message Structure:
no details available
- Constraint:
t_Dly (1000 Ms)
- BinaryMessage:

- No.: 1017
- Timestamp: 20:28:37:475_0
- RFN: 1319
- Chip: 19456
- Event: Timeout
- Source: ts_RRC_Delay LINE 2
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 1022
- Timestamp: 20:28:37:480_0
- RFN: 1320
- Chip: 1536
- Event: Send
- PCO: UM
- Message: RLC_UM_DATA_REQ
- Source: ts_RRC_ConnRel:lt_Send_RRC_ConnectionRelease LINE 3
- Message Structure:
RLC_UM_DATA_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. uM_message
. . DL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00000000000000000000000000000000"
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . DL_DCCH_MessageType
. . . . RRCConnectionRelease
. . . . . r3
. . . . . . RRCConnectionRelease_r3_IEs
. . . . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . . . (IntegerType)n_308 = 1
. . . . . . . (ReleaseCause)releaseCause = 0
. . . . . . . Rplmn_Information
. . . . . . laterNonCriticalExtensions
. (BooleanType)specialLI = FALSE
- Constraint:
cas_RRC_ConnRelDCCH
- BinaryMessage:
30 10 02 01 ff 02 01 01 80 00 00 00 03 c8 00 01 01 00

- No.: 1026
- Timestamp: 20:28:37:612_0
- RFN: 1333
- Chip: 9216
- Event: Receive
- PCO: UM
- Message: RLC_UM_DATA_IND
- Source: ts_RRC_ConnRel:lt_Send_RRC_ConnectionRelease LINE 4
- Message Structure:
RLC_UM_DATA_IND
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. IntegrityResult
. uM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "10101101101011101001000000111001"
. . . . (IntegerType)rrc_MessageSequenceNumber = 1
. . . UL_DCCH_MessageType
. . . . RRCConnectionReleaseComplete
. . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . FailureCauseWithProtErr
. . . . . laterNonCriticalExtensions
. . . . . . (BitStringType)rrcConnectionReleaseComplete_r3_add_ext = 0
. . . . . . nonCriticalExtensions
- Constraint:
car_RRC_ConnRelCmplUM
- BinaryMessage:
30 0c 02 01 ff 02 01 01 d6 d7 48 1c 8c 40

- No.: 1027
- Timestamp: 20:28:37:613_0
- RFN: 1333
- Chip: 12800
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ConnRel:lt_Send_RRC_ConnectionRelease LINE 4
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1030
- Timestamp: 20:28:37:614_2
- RFN: 1333
- Chip: 17920
- Event: Start Timer
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 1
- Message Structure:
no details available
- Constraint:
t_Dly (5000 Ms)
- BinaryMessage:

- No.: 1034
- Timestamp: 20:28:37:772_0
- RFN: 1349
- Chip: 8192
- Event: Receive
- PCO: UM
- Message: RLC_UM_DATA_IND
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 4
- Message Structure:
RLC_UM_DATA_IND
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. IntegrityResult
. uM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00011100010101000111110101101001"
. . . . (IntegerType)rrc_MessageSequenceNumber = 2
. . . UL_DCCH_MessageType
. . . . RRCConnectionReleaseComplete
. . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . FailureCauseWithProtErr
. . . . . laterNonCriticalExtensions
. . . . . . (BitStringType)rrcConnectionReleaseComplete_r3_add_ext = 0
. . . . . . nonCriticalExtensions
- Constraint:
car_RRC_ConnRelCmplUM
- BinaryMessage:
30 0c 02 01 ff 02 01 01 8e 2a 3e b4 94 40

- No.: 1035
- Timestamp: 20:28:37:773_0
- RFN: 1349
- Chip: 11776
- Event: Cancel Timer
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 4
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 1036
- Timestamp: 20:28:37:774_0
- RFN: 1349
- Chip: 13056
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 4
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1042
- Timestamp: 20:28:37:777_0
- RFN: 1349
- Chip: 27648
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 01 0a 01 00 05 00

- No.: 1046
- Timestamp: 20:28:37:783_0
- RFN: 1350
- Chip: 13056
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 1049
- Timestamp: 20:28:37:786_0
- RFN: 1350
- Chip: 23552
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 02 0a 01 00 05 00

- No.: 1053
- Timestamp: 20:28:37:794_0
- RFN: 1351
- Chip: 16384
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 1056
- Timestamp: 20:28:37:797_0
- RFN: 1351
- Chip: 27648
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 03 0a 01 00 05 00

- No.: 1060
- Timestamp: 20:28:37:807_0
- RFN: 1352
- Chip: 26880
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 1063
- Timestamp: 20:28:37:810_0
- RFN: 1352
- Chip: 37888
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 04 0a 01 00 05 00

- No.: 1067
- Timestamp: 20:28:37:821_0
- RFN: 1354
- Chip: 3584
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 1070
- Timestamp: 20:28:37:828_0
- RFN: 1354
- Chip: 30720
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 136
. . . . . UL_RLC_Mode
. . . . . . UL_UM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (NoExplicitDiscard)timerBasedNoExplicit = 9
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = 1
. . . . (IntegerType)dLlogicalChannelIdentity = 1
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_UM_Info
- BinaryMessage:
30 22 02 01 ff 02 01 01 0a 01 00 30 17 30 0d 05 00 30 09 02 02 00 88 30 03 0a 01 09 30 06 02 01 01 02 01 01

- No.: 1074
- Timestamp: 20:28:37:839_0
- RFN: 1355
- Chip: 34048
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 1075
- Timestamp: 20:28:37:847_0
- RFN: 1356
- Chip: 28160
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 3
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . (TimerEPC)timerEPC = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . (TimerRST)timerRST = 9
. . . . . . . (MaxRST)max_RST = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = 2
. . . . (IntegerType)dLlogicalChannelIdentity = 2
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 02 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 27 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 02 02 01 02

- No.: 1079
- Timestamp: 20:28:37:869_0
- RFN: 1358
- Chip: 34816
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 4
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 1080
- Timestamp: 20:28:37:878_0
- RFN: 1359
- Chip: 31744
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 5
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . (TimerEPC)timerEPC = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . (TimerRST)timerRST = 9
. . . . . . . (MaxRST)max_RST = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = 3
. . . . (IntegerType)dLlogicalChannelIdentity = 3
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 03 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 27 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 03 02 01 03

- No.: 1084
- Timestamp: 20:28:37:894_0
- RFN: 1361
- Chip: 16384
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 6
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 1085
- Timestamp: 20:28:37:903_0
- RFN: 1362
- Chip: 12288
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 7
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . (TimerEPC)timerEPC = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . (TimerRST)timerRST = 9
. . . . . . . (MaxRST)max_RST = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = 4
. . . . (IntegerType)dLlogicalChannelIdentity = 4
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 04 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 27 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 04 02 01 04

- No.: 1089
- Timestamp: 20:28:37:928_0
- RFN: 1364
- Chip: 33536
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 8
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 1112
- Timestamp: 20:28:37:936_0
- RFN: 1365
- Chip: 24064
- Event: Start Timer
- Source: ts_GMM_IdleUpdated:lt_HandleAttachRequest LINE 5
- Message Structure:
no details available
- Constraint:
t_WaitS (1 Sec)
- BinaryMessage:

- No.: 1116
- Timestamp: 20:28:38:940_0
- RFN: 1466
- Chip: 2816
- Event: Timeout
- Source: ts_GMM_IdleUpdated:lt_HandleAttachRequest LINE 6
- Message Structure:
no details available
- Constraint:
t_WaitS
- BinaryMessage:

- No.: 1118
- Timestamp: 20:28:38:941_0
- RFN: 1466
- Chip: 5376
- Event: Start Timer
- Source: ts_GMM_IdleUpdated:lt_HandleAttachRequest LINE 7
- Message Structure:
no details available
- Constraint:
t_WaitS (60 Sec)
- BinaryMessage:

- No.: 1120
- Timestamp: 20:28:38:943_0
- RFN: 1466
- Chip: 13312
- Event: Send
- PCO: Ut
- Message: AT_CmdReq
- Source: ts_AT_TriggerGMM_Attach LINE 1
- Message Structure:
AT_CmdReq
. (IA5StringType)cmd[-1] = "AT+CGATT=1"
. (HexStringType)sMS_BlockMode[-1] = -
- Constraint:
ca_AT_CmdReq
- BinaryMessage:
41 54 2b 43 47 41 54 54 3d 31 3c 43 52 3e

- No.: 1124
- Timestamp: 20:28:40:069_0
- RFN: 1578
- Chip: 35584
- Event: Receive
- PCO: Ut
- Message: AT_CmdCnf
- Source: ts_AT_TriggerGMM_Attach LINE 2
- Message Structure:
AT_CmdCnf
. (BooleanType)result = TRUE
. (IA5StringType)resultString[18] = "OK"
. (HexStringType)sMS_BlockMode[0] = -
- Constraint:
ca_AT_CmdCnf
- BinaryMessage:
80 3c 43 52 3e 3c 4c 46 3e 4f 4b 3c 43 52 3e 3c 4c 46 3e

- No.: 1141
- Timestamp: 20:28:40:076_0
- RFN: 1579
- Chip: 22784
- Event: Receive
- PCO: CPHY
- Message: CPHY_Out_of_Sync_IND
- Source: RRC_DefConnEst LINE 7
- Message Structure:
CPHY_Out_of_Sync_IND
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_OutOfSyncInd
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 1142
- Timestamp: 20:28:40:076_1
- RFN: 1579
- Chip: 24576
- Event: Cancel Timer
- Source: RRC_DefConnEst LINE 7
- Message Structure:
no details available
- Constraint:
t_T312
- BinaryMessage:

- No.: 1143
- Timestamp: 20:28:40:077_0
- RFN: 1579
- Chip: 26624
- Event: Default
- Source: RRC_DefConnEst LINE 0
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1144
- Timestamp: 20:28:40:077_1
- RFN: 1579
- Chip: 27392
- Event: Default
- Source: ts_RRC_ConnEst:lt_RcvConnReq LINE 2
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1149
- Timestamp: 20:28:45:725_0
- RFN: 2144
- Chip: 18688
- Event: Receive
- PCO: TM
- Message: RLC_TR_DATA_IND
- Source: ts_RRC_ConnEst:lt_RcvConnReq LINE 2
- Message Structure:
RLC_TR_DATA_IND
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
. tM_message
. . UL_CCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode = 0
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . UL_CCCH_MessageType
. . . . RRCConnectionRequest
. . . . . InitialUE_Identity
. . . . . . TMSI_and_LAI_GSM_MAP
. . . . . . . (BitStringType)tmsi[32] = "00010010001101000101011001111000"
. . . . . . . LAI
. . . . . . . . PLMN_Identity
. . . . . . . . . MCC
. . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . (IntegerType)_elem = 1
. . . . . . . . . MNC
. . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . (IntegerType)_elem = 1
. . . . . . . . (BitStringType)lac[16] = '0000000000000001'B
. . . . . (EstablishmentCause)establishmentCause = 12
. . . . . (ProtocolErrorIndicator)protocolErrorIndicator = 0
. . . . . MeasuredResultsOnRACH
. . . . . . currentCell
. . . . . . . modeSpecificInfo
. . . . . . . . fdd
. . . . . . . . . measurementQuantity
. . . . . . . . . . (IntegerType)cpich_Ec_N0 = 0
. . . . . v3d0NonCriticalExtensions
. . . . . . RRCConnectionRequest_v3d0ext_IEs
. . . . . . . (BitStringType)uESpecificBehaviourInformation1idle = 0
. . . . . . nonCriticalExtensions
- Constraint:
car_RRC_ConnReq
- BinaryMessage:
30 11 02 01 00 02 01 00 21 12 34 56 78 00 10 08 00 0b 00

- No.: 1153
- Timestamp: 20:28:45:785_0
- RFN: 2150
- Chip: 21760
- Event: Send
- PCO: UM
- Message: RLC_UM_DATA_REQ
- Source: ts_RRC_ConnEst:lt_Send_ConnSetUp LINE 22
- Message Structure:
RLC_UM_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
. uM_message
. . DL_CCCH_Message
. . . IntegrityCheckInfo
. . . DL_CCCH_MessageType
. . . . RRCConnectionSetup
. . . . . r3
. . . . . . RRCConnectionSetup_r3_IEs
. . . . . . . InitialUE_Identity
. . . . . . . . TMSI_and_LAI_GSM_MAP
. . . . . . . . . (BitStringType)tmsi[32] = "00010010001101000101011001111000"
. . . . . . . . . LAI
. . . . . . . . . . PLMN_Identity
. . . . . . . . . . . MCC
. . . . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . . . (IntegerType)_elem = 1
. . . . . . . . . . . MNC
. . . . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . . . (IntegerType)_elem = 1
. . . . . . . . . . (BitStringType)lac[16] = '0000000000000001'B
. . . . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . . . (IntegerType)activationTime = -
. . . . . . . U_RNTI
. . . . . . . . (BitStringType)srnc_Identity[12] = "000000000001"
. . . . . . . . (BitStringType)s_RNTI[20] = "00000000000000000001"
. . . . . . . (BitStringType)new_c_RNTI[16] = -
. . . . . . . (RRC_StateIndicator)rrc_StateIndicator = 0
. . . . . . . (IntegerType)utran_DRX_CycleLengthCoeff = 9
. . . . . . . CapabilityUpdateRequirement
. . . . . . . . (BooleanType)ue_RadioCapabilityFDDUpdateRequirement = TRUE
. . . . . . . . (BooleanType)ue_RadioCapabilityTDDUpdateRequirement = FALSE
. . . . . . . . SystemSpecificCapUpdateReqList
. . . . . . . . . (SystemSpecificCapUpdateReq)_elem = 0
. . . . . . . SRB_InformationSetupList2
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_UM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 1
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 1
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . . . . . . . (TimerRST)timerRST = 9
. . . . . . . . . . . . . (MaxRST)max_RST = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 2
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 2
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . . . . . . . (TimerRST)timerRST = 9
. . . . . . . . . . . . . (MaxRST)max_RST = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 3
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 3
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . . . . . . . (TimerRST)timerRST = 9
. . . . . . . . . . . . . (MaxRST)max_RST = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 4
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 4
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . UL_CommonTransChInfo
. . . . . . . . TFC_Subset
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . TFCS
. . . . . . . . . . . ExplicitTFCS_Configuration
. . . . . . . . . . . . TFCS_ReconfAdd
. . . . . . . . . . . . . ctfcSize
. . . . . . . . . . . . . . ctfc2Bit
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . . . . . . . (IntegerType)ctfc2 = 0
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . . . . . . . (IntegerType)ctfc2 = 1
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 11
. . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . UL_AddReconfTransChInfoList
. . . . . . . . UL_AddReconfTransChInformation
. . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType = 0
. . . . . . . . . (IntegerType)transportChannelIdentity = 5
. . . . . . . . . TransportFormatSet
. . . . . . . . . . DedicatedTransChTFS
. . . . . . . . . . . tti
. . . . . . . . . . . . DedicatedDynamicTF_InfoList
. . . . . . . . . . . . . DedicatedDynamicTF_Info
. . . . . . . . . . . . . . rlc_Size
. . . . . . . . . . . . . . . BitModeRLC_SizeInfo
. . . . . . . . . . . . . . . . sizeType2
. . . . . . . . . . . . . . . . . (IntegerType)part1 = 2
. . . . . . . . . . . . . . . . . (IntegerType)part2 = -
. . . . . . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . LogicalChannelList
. . . . . . . . . . . SemistaticTF_Information
. . . . . . . . . . . . ChannelCodingType
. . . . . . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . . . . . (IntegerType)rateMatchingAttribute = 192
. . . . . . . . . . . . (CRC_Size)crc_Size = 3
. . . . . . . DL_CommonTransChInfo
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . dl_Parameters
. . . . . . . DL_AddReconfTransChInfoList
. . . . . . . . DL_AddReconfTransChInformation
. . . . . . . . . (DL_TrCH_Type)dl_TransportChannelType = 0
. . . . . . . . . (IntegerType)dl_transportChannelIdentity = 10
. . . . . . . . . tfs_SignallingMode
. . . . . . . . . . UL_TransportChannelIdentity
. . . . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType = 0
. . . . . . . . . . . (IntegerType)ul_TransportChannelIdentity = 5
. . . . . . . . . QualityTarget
. . . . . . . . . . (IntegerType)bler_QualityValue = -20
. . . . . . . . . TM_SignallingInfo
. . . . . . . FrequencyInfo
. . . . . . . (IntegerType)maxAllowedUL_TX_Power = -
. . . . . . . UL_ChannelRequirement
. . . . . . . . UL_DPCH_Info
. . . . . . . . . UL_DPCH_PowerControlInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (IntegerType)dpcch_PowerOffset = -40
. . . . . . . . . . . (IntegerType)pc_Preamble = 1
. . . . . . . . . . . (IntegerType)sRB_delay = 7
. . . . . . . . . . . PowerControlAlgorithm
. . . . . . . . . . . . (IntegerType)algorithm1 = 1
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (ScramblingCodeType)scramblingCodeType = 1
. . . . . . . . . . . (IntegerType)scramblingCode = 0
. . . . . . . . . . . (IntegerType)numberOfDPDCH = -
. . . . . . . . . . . (SpreadingFactor)spreadingFactor = 4
. . . . . . . . . . . (BooleanType)tfci_Existence = TRUE
. . . . . . . . . . . (IntegerType)numberOfFBI_Bits = -
. . . . . . . . . . . (PuncturingLimit)puncturingLimit = 15
. . . . . . . DL_CommonInformation
. . . . . . . . DL_DPCH_InfoCommon
. . . . . . . . . cfnHandling
. . . . . . . . . . initialise
. . . . . . . . . . . (IntegerType)cfntargetsfnframeoffset = -
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . DL_DPCH_PowerControlInfo
. . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . (DPC_Mode)dpc_Mode = 0
. . . . . . . . . . . (IntegerType)powerOffsetPilot_pdpdch = 0
. . . . . . . . . . . Dl_rate_matching_restriction
. . . . . . . . . . . SF512_AndPilot
. . . . . . . . . . . . (PilotBits128)sfd128 = 0
. . . . . . . . . . . (PositionFixedOrFlexible)positionFixedOrFlexible = 0
. . . . . . . . . . . (BooleanType)tfci_Existence = FALSE
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . (IntegerType)defaultDPCH_OffsetValue = 0
. . . . . . . . . . DPCH_CompressedModeInfo
. . . . . . . . . . (TX_DiversityMode)tx_DiversityMode = 0
. . . . . . . . . . SSDT_Information
. . . . . . . DL_InformationPerRL_List
. . . . . . . . DL_InformationPerRL
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . PrimaryCPICH_Info
. . . . . . . . . . . . (IntegerType)primaryScramblingCode = 100
. . . . . . . . . . . PDSCH_SHO_DCH_Info
. . . . . . . . . . . PDSCH_CodeMapping
. . . . . . . . . DL_DPCH_InfoPerRL
. . . . . . . . . . fdd
. . . . . . . . . . . (PCPICH_UsageForChannelEst)pCPICH_UsageForChannelEst = 0
. . . . . . . . . . . (IntegerType)dpch_FrameOffset = 0
. . . . . . . . . . . SecondaryCPICH_Info
. . . . . . . . . . . DL_ChannelisationCodeList
. . . . . . . . . . . . DL_ChannelisationCode
. . . . . . . . . . . . . (IntegerType)secondaryScramblingCode = 1
. . . . . . . . . . . . . SF512_AndCodeNumber
. . . . . . . . . . . . . . (IntegerType)sf128 = 0
. . . . . . . . . . . . . (ScramblingCodeChange)scramblingCodeChange = 1
. . . . . . . . . . . (IntegerType)tpc_CombinationIndex = 0
. . . . . . . . . . . (SSDT_CellIdentity)ssdt_CellIdentity = -
. . . . . . . . . . . (ClosedLoopTimingAdjMode)closedLoopTimingAdjMode = -
. . . . . . . . . SCCPCH_InfoForFACH
. . . . . . laterNonCriticalExtensions
. (BooleanType)specialLI = TRUE
- Constraint:
cas_RRC_ConnSetup
- BinaryMessage:
30 78 02 01 00 02 01 00 30 e7 22 46 8a cf 00 02 01 00 01 00 04 00 00 4d 82 69 3a 10 10 89 0d 42 00 02 81 9e 8e 46 c9 ce 7c 9c 4e 74 20 a5 12 3a 8c 00 15 13 3d 1c 8d 93 9c f9 38 9c e8 42 52 24 b5 28 00 4a 46 7a 39 1b 27 39 f2 71 39 d0 86 b4 49 ea 70 00 d4 c8 00 06 25 2b f0 02 00 08 82 23 bf 66 08 98 95 a5 47 a2 00 00 01 3f 90 0a 14 00 02 06 40 00 0c 28 08 01 01 ff

- No.: 1174
- Timestamp: 20:28:45:828_2
- RFN: 2154
- Chip: 34304
- Event: Start Timer
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 3
- Message Structure:
no details available
- Constraint:
t_WaitMS (13500 Ms)
- BinaryMessage:

- No.: 1179
- Timestamp: 20:28:46:038_0
- RFN: 2175
- Chip: 31744
- Event: Receive
- PCO: CPHY
- Message: CPHY_Sync_IND
- Source: RRC_Def1 LINE 13
- Message Structure:
CPHY_Sync_IND
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_SyncInd
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 1180
- Timestamp: 20:28:46:038_1
- RFN: 2175
- Chip: 33536
- Event: Cancel Timer
- Source: RRC_Def1 LINE 13
- Message Structure:
no details available
- Constraint:
t_T312
- BinaryMessage:

- No.: 1181
- Timestamp: 20:28:46:039_0
- RFN: 2175
- Chip: 35072
- Event: Default
- Source: RRC_Def1 LINE 0
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1182
- Timestamp: 20:28:46:039_1
- RFN: 2175
- Chip: 35840
- Event: Default
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1187
- Timestamp: 20:28:46:152_0
- RFN: 2187
- Chip: 11520
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_IND
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
RLC_AM_DATA_IND
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. IntegrityResult
. . (IntegrityStatus)integrityUsed = 0
. aM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode = 0
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . UL_DCCH_MessageType
. . . . RRCConnectionSetupComplete
. . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . STARTList
. . . . . . STARTSingle
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity = 1
. . . . . . . (BitStringType)start_Value[20] = "00000000000000000100"
. . . . . . STARTSingle
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity = 0
. . . . . . . (BitStringType)start_Value[20] = "00000000000000000010"
. . . . . UE_RadioAccessCapability
. . . . . . (AccessStratumReleaseIndicator)accessStratumReleaseIndicator = 0
. . . . . . PDCP_Capability
. . . . . . . (BooleanType)losslessSRNS_RelocationSupport = FALSE
. . . . . . . supportForRfc2507
. . . . . . RLC_Capability
. . . . . . . (TotalRLC_AM_BufferSize)totalRLC_AM_BufferSize = 2
. . . . . . . (MaximumRLC_WindowSize)maximumRLC_WindowSize = 0
. . . . . . . (MaximumAM_EntityNumberRLC_Cap)maximumAM_EntityNumber = 3
. . . . . . TransportChannelCapability
. . . . . . . DL_TransChCapability
. . . . . . . . (MaxNoBits)maxNoBitsReceived = 4
. . . . . . . . (MaxNoBits)maxConvCodeBitsReceived = 1
. . . . . . . . TurboSupport
. . . . . . . . . (MaxNoBits)supported = 4
. . . . . . . . (MaxSimultaneousTransChsDL)maxSimultaneousTransChs = 1
. . . . . . . . (IntegerType)maxSimultaneousCCTrCH_Count = 1
. . . . . . . . (MaxTransportBlocksDL)maxReceivedTransportBlocks = 2
. . . . . . . . (MaxNumberOfTFC_DL)maxNumberOfTFC = 4
. . . . . . . . (MaxNumberOfTF)maxNumberOfTF = 1
. . . . . . . UL_TransChCapability
. . . . . . . . (MaxNoBits)maxNoBitsTransmitted = 3
. . . . . . . . (MaxNoBits)maxConvCodeBitsTransmitted = 1
. . . . . . . . TurboSupport
. . . . . . . . . (MaxNoBits)supported = 3
. . . . . . . . (MaxSimultaneousTransChsUL)maxSimultaneousTransChs = 2
. . . . . . . . modeSpecificInfo
. . . . . . . . (MaxTransportBlocksUL)maxTransmittedBlocks = 2
. . . . . . . . (MaxNumberOfTFC_UL)maxNumberOfTFC = 3
. . . . . . . . (MaxNumberOfTF)maxNumberOfTF = 0
. . . . . . RF_Capability
. . . . . . . fddRF_Capability
. . . . . . . . (IntegerType)ue_PowerClass = 4
. . . . . . . . (TxRxFrequencySeparation)txRxFrequencySeparation = 0
. . . . . . . tddRF_Capability
. . . . . . . . (IntegerType)ue_PowerClass = 0
. . . . . . . . (RadioFrequencyBandTDDList)radioFrequencyTDDBandList = 0
. . . . . . . . (ChipRateCapability)chipRateCapability = 0
. . . . . . PhysicalChannelCapability
. . . . . . . fddPhysChCapability
. . . . . . . . DL_PhysChCapabilityFDD
. . . . . . . . . (IntegerType)maxNoDPCH_PDSCH_Codes = 3
. . . . . . . . . (MaxNoPhysChBitsReceived)maxNoPhysChBitsReceived = 6
. . . . . . . . . (BooleanType)supportForSF_512 = FALSE
. . . . . . . . . (BooleanType)supportOfPDSCH = FALSE
. . . . . . . . . SimultaneousSCCPCH_DPCH_Reception
. . . . . . . . UL_PhysChCapabilityFDD
. . . . . . . . . (MaxNoDPDCH_BitsTransmitted)maxNoDPDCH_BitsTransmitted = 2
. . . . . . . . . (BooleanType)supportOfPCPCH = FALSE
. . . . . . . tddPhysChCapability
. . . . . . . . DL_PhysChCapabilityTDD
. . . . . . . . . (IntegerType)maxTS_PerFrame = 0
. . . . . . . . . (IntegerType)maxPhysChPerFrame = 0
. . . . . . . . . (MinimumSF_DL)minimumSF = 0
. . . . . . . . . (BooleanType)supportOfPDSCH = FALSE
. . . . . . . . . (IntegerType)maxPhysChPerTS = 0
. . . . . . . . UL_PhysChCapabilityTDD
. . . . . . . . . (IntegerType)maxTS_PerFrame = 0
. . . . . . . . . (MaxPhysChPerTimeslot)maxPhysChPerTimeslot = 0
. . . . . . . . . (MinimumSF_UL)minimumSF = 0
. . . . . . . . . (BooleanType)supportOfPUSCH = FALSE
. . . . . . UE_MultiModeRAT_Capability
. . . . . . . MultiRAT_Capability
. . . . . . . . (BooleanType)supportOfGSM = TRUE
. . . . . . . . (BooleanType)supportOfMulticarrier = FALSE
. . . . . . . (MultiModeCapability)multiModeCapability = 1
. . . . . . SecurityCapability
. . . . . . . (BitStringType)cipheringAlgorithmCap[16] = '0000000000000011'B
. . . . . . . (BitStringType)integrityProtectionAlgorithmCap[16] = '0000000000000010'B
. . . . . . UE_Positioning_Capability
. . . . . . . (BooleanType)standaloneLocMethodsSupported = FALSE
. . . . . . . (BooleanType)ue_BasedOTDOA_Supported = FALSE
. . . . . . . (NetworkAssistedGPS_Supported)networkAssistedGPS_Supported = 3
. . . . . . . (BooleanType)supportForUE_GPS_TimingOfCellFrames = FALSE
. . . . . . . (BooleanType)supportForIPDL = FALSE
. . . . . . MeasurementCapability
. . . . . . . CompressedModeMeasCapability
. . . . . . . . (BooleanType)fdd_Measurements = TRUE
. . . . . . . . (BooleanType)tdd_Measurements = FALSE
. . . . . . . . GSM_Measurements
. . . . . . . . . (BooleanType)gsm900 = TRUE
. . . . . . . . . (BooleanType)dcs1800 = TRUE
. . . . . . . . . (BooleanType)gsm1900 = FALSE
. . . . . . . . (BooleanType)multiCarrierMeasurements = FALSE
. . . . . . . CompressedModeMeasCapability
. . . . . . . . (BooleanType)fdd_Measurements = TRUE
. . . . . . . . (BooleanType)tdd_Measurements = FALSE
. . . . . . . . GSM_Measurements
. . . . . . . . . (BooleanType)gsm900 = TRUE
. . . . . . . . . (BooleanType)dcs1800 = TRUE
. . . . . . . . . (BooleanType)gsm1900 = FALSE
. . . . . . . . (BooleanType)multiCarrierMeasurements = FALSE
. . . . . v370NonCriticalExtensions
. . . . . . RRCConnectionSetupComplete_v370ext
. . . . . . . UE_RadioAccessCapability_v370ext
. . . . . . v380NonCriticalExtensions
. . . . . . . RRCConnectionSetupComplete_v380ext_IEs
. . . . . . . . UE_RadioAccessCapability_v380ext
. . . . . . . . . UE_PositioningCapabilityExt_v380
. . . . . . . . . . (BooleanType)rx_tx_TimeDifferenceType2Capable = FALSE
. . . . . . . . DL_PhysChCapabilityFDD_v380ext
. . . . . . . . . (SupportOfDedicatedPilotsForChEstimation)supportOfDedicatedPilotsForChEstimation = 0
. . . . . . . v3a0NonCriticalExtensions
. . . . . . . . RRCConnectionSetupComplete_v3a0ext_IEs
. . . . . . . . . UE_RadioAccessCapability_v3a0ext
. . . . . . . . . . UE_PositioningCapabilityExt_v3a0
. . . . . . . . . . . (UE_PositioningCapabilityExt_v3a0_list_0)validity_CellPCH_UraPCH = 0
. . . . . . . . laterNonCriticalExtensions
. . . . . . . . . (BitStringType)rrcConnectionSetupComplete_r3_add_ext = 0
. . . . . . . . . nonCriticalExtensions
- Constraint:
car_RRC_ConnSetupCmpl
- BinaryMessage:
30 27 02 01 ff 02 01 02 0a 05 01 00 00 00 00 4a 0c 00 01 00 00 05 11 a0 d1 04 84 c6 68 46 2c 93 02 48 00 18 00 11 8f 8f 80

- No.: 1188
- Timestamp: 20:28:46:161_0
- RFN: 2188
- Chip: 3072
- Event: Cancel Timer
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
t_WaitMS
- BinaryMessage:

- No.: 1189
- Timestamp: 20:28:46:161_1
- RFN: 2188
- Chip: 4608
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1203
- Timestamp: 20:28:46:170_0
- RFN: 2189
- Chip: 256
- Event: Send
- PCO: CMAC
- Message: CMAC_SecurityMode_Config_REQ
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 1
- Message Structure:
CMAC_SecurityMode_Config_REQ
. (IntegerType)cellId = 0
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity = 1
. . (BitStringType)startValue[20] = "00000000000000000100"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = -
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CMAC_SecurityModeCfgReq
- BinaryMessage:
30 0e 02 01 00 30 09 0a 01 01 03 04 04 00 00 40

- No.: 1204
- Timestamp: 20:28:46:173_0
- RFN: 2189
- Chip: 8704
- Event: Receive
- PCO: CMAC
- Message: CMAC_SecurityMode_Config_CNF
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 2
- Message Structure:
CMAC_SecurityMode_Config_CNF
. (IntegerType)cellId = 0
- Constraint:
ca_CMAC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 00

- No.: 1205
- Timestamp: 20:28:46:174_0
- RFN: 2189
- Chip: 16128
- Event: Send
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_REQ
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 3
- Message Structure:
CRLC_SecurityMode_Config_REQ
. (IntegerType)cellId = -1
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity = 1
. . (BitStringType)startValue[20] = "00000000000000000100"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = -
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CRLC_SecurityModeCfgReq
- BinaryMessage:
30 0e 02 01 ff 30 09 0a 01 01 03 04 04 00 00 40

- No.: 1206
- Timestamp: 20:28:46:176_0
- RFN: 2189
- Chip: 22272
- Event: Receive
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_CNF
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 4
- Message Structure:
CRLC_SecurityMode_Config_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1220
- Timestamp: 20:28:46:181_0
- RFN: 2190
- Chip: 2816
- Event: Send
- PCO: CMAC
- Message: CMAC_SecurityMode_Config_REQ
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 1
- Message Structure:
CMAC_SecurityMode_Config_REQ
. (IntegerType)cellId = 0
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity = 0
. . (BitStringType)startValue[20] = "00000000000000000010"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = -
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CMAC_SecurityModeCfgReq
- BinaryMessage:
30 0e 02 01 00 30 09 0a 01 00 03 04 04 00 00 20

- No.: 1221
- Timestamp: 20:28:46:183_0
- RFN: 2190
- Chip: 9984
- Event: Receive
- PCO: CMAC
- Message: CMAC_SecurityMode_Config_CNF
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 2
- Message Structure:
CMAC_SecurityMode_Config_CNF
. (IntegerType)cellId = 0
- Constraint:
ca_CMAC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 00

- No.: 1222
- Timestamp: 20:28:46:185_0
- RFN: 2190
- Chip: 17152
- Event: Send
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_REQ
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 3
- Message Structure:
CRLC_SecurityMode_Config_REQ
. (IntegerType)cellId = -1
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity = 0
. . (BitStringType)startValue[20] = "00000000000000000010"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = -
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CRLC_SecurityModeCfgReq
- BinaryMessage:
30 0e 02 01 ff 30 09 0a 01 00 03 04 04 00 00 20

- No.: 1223
- Timestamp: 20:28:46:186_0
- RFN: 2190
- Chip: 23296
- Event: Receive
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_CNF
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 4
- Message Structure:
CRLC_SecurityMode_Config_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1230
- Timestamp: 20:28:46:195_0
- RFN: 2191
- Chip: 20224
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_GMM_IdleUpdated:lt_HandleAttachRequest LINE 10
- Message Structure:
RRC_DataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. (START_Value)start[20] = '00000000000000000100'B
. ATTACHREQUEST
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)gMMProtocolDiscriminator[4] = '1000'B
. . (MsgType)msgType[8] = '00000001'B
. . MS_NetworkCap_lv
. . . (Length)iel[1] = '02'O
. . . (OctetStringType)value[2] = 'E540'O
. . CiphKeySeqNum
. . . (B1)spare1[1] = '0'B
. . . (KeySeq)keySeq[3] = '000'B
. . AttachType
. . . (B1)pre_for[1] = '0'B
. . . (B3)type[3] = '001'B
. . DRXparamter
. . . (B8)splitPGcycleCode[8] = '00000111'B
. . . (B4)cnDRXcoef[4] = '0000'B
. . . (B1)splitOnCCCH[1] = '0'B
. . . (B3)nonDRXtimer[3] = '010'B
. . MS_Identity_lv
. . . (Length)iel[1] = '05'O
. . . (B4)iDigit1[4] = '1111'B
. . . (B1)oddEvenInd[1] = '0'B
. . . (B3)typeOfId[3] = '100'B
. . . (OctetStringType)otherDigits[4] = '12345678'O
. . RAI_v
. . . (OctetStringType)plmn[3] = '00F110'O
. . . (OctetStringType)lac[2] = '0001'O
. . . (OctetStringType)rac[1] = '05'O
. . MSRadioAccessCap_lv
. . . (Length)iel[1] = '0A'O
. . . (OctetStringType)value[10] = '14F382334C03263CA060'O
. . PTMSI_Signature
. . . (IEI8)iei[8] = '00010111'B
. . . (OctetStringType)value[3] = -
. . GPRS_Timer
. . . (IEI8)iei[8] = '00010110'B
. . . (B3)unit[0] = -
. . . (B5)value[0] = -
. . TMSI_Status
. . . (IEI4)iei[0] = -
. . . (B3)spare3[0] = -
. . . (B1)flag[0] = -
- Constraint:
car_PS_InitDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 03 04 04 00 00 40 08 01 02 e5 40 01 07 02 05 f4 12 34 56 78 00 f1 10 00 01 05 0a 14 f3 82 33 4c 03 26 3c a0 60 17 16

- No.: 1231
- Timestamp: 20:28:46:200_0
- RFN: 2192
- Chip: 1280
- Event: Cancel Timer
- Source: ts_GMM_IdleUpdated:lt_HandleAttachRequest LINE 10
- Message Structure:
no details available
- Constraint:
t_WaitS
- BinaryMessage:

- No.: 1268
- Timestamp: 20:28:46:217_0
- RFN: 2193
- Chip: 27136
- Event: Send
- PCO: Dc
- Message: RRC_DataReq
- Source: ts_GMM_Authentication LINE 2
- Message Structure:
RRC_DataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[-1] = -
. (SapId)sapId[1] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. AUTHENTICATIONANDCIPHERINGREQUEST
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)gMMProtocolDiscriminator[4] = '1000'B
. . (MsgType)msgType[8] = '00010010'B
. . IMEISVRequest
. . . (B1)spare1[1] = '0'B
. . . (B3)value[3] = '000'B
. . CiphAlgorithm
. . . (B1)spare1[1] = '0'B
. . . (B3)algorithm[3] = '001'B
. . AC_ReferenceNumber
. . . (B4)value[4] = '0011'B
. . ForceToStandby
. . . (B1)spare[1] = '0'B
. . . (B3)value[3] = '000'B
. . AuthenticationParamterRAND
. . . (IEI8)iei[8] = '00100001'B
. . . (BitStringType)randValue[128] = '01010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101'B
. . CiphKeySeqNum_tv
. . . (IEI4)iei[4] = '1000'B
. . . (B1)spare1[1] = '0'B
. . . (KeySeq)keySeq[3] = '000'B
. . GMM_AUTN
. . . (IEI8)iei[8] = '00101000'B
. . . (Length)iel[1] = '10'O
. . . (BitStringType)aUTN[128] = '01010110010100010101000001010011010100100101110100000000000000000101010101010100010101110101011001010001010100000101001101010010'B
- Constraint:
ca_PS_DataReq
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 08 12 01 30 21 55 55 55 55 55 55 55 55 55 55 55 55 55 55 55 55 80 28 10 56 51 50 53 52 5d 00 00 55 54 57 56 51 50 53 52

- No.: 1272
- Timestamp: 20:28:46:876_0
- RFN: 2259
- Chip: 24576
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_GMM_Authentication LINE 7
- Message Structure:
RRC_DataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. (START_Value)start[0] = -
. AUTHENTICATIONANDCIPHERINGRESPONSE
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)gMMProtocolDiscriminator[4] = '1000'B
. . (MsgType)msgType[8] = '00010011'B
. . (B4)spare4[4] = '0000'B
. . AC_ReferenceNumber
. . . (B4)value[4] = '0011'B
. . AuthRsp_tv
. . . (IEI8)iei[8] = '00100010'B
. . . (BitStringType)value[32] = '01010101010101000101011101010110'B
. . GMM_MS_Identity
. . AuthRspExt
- Constraint:
car_PS_UplinkDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 08 13 03 22 55 54 57 56

- No.: 1275
- Timestamp: 20:28:46:879_1
- RFN: 2259
- Chip: 33792
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_GMM_Authentication LINE 10
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1312
- Timestamp: 20:28:46:892_0
- RFN: 2261
- Chip: 6144
- Event: Send
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_REQ
- Source: ts_SS_DownloadSecurityKey:lt_DownloadKeyCRLC LINE 1
- Message Structure:
CRLC_SecurityMode_Config_REQ
. (IntegerType)cellId = -1
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity = 1
. . (BitStringType)startValue[20] = "00000000000000000000"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = '01010111010101100101000101010000010100110101001001011101010111000101111101011110010110010101100001011011010110100101010101010100'B
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CRLC_SecurityModeCfgReq
- BinaryMessage:
30 21 02 01 ff 30 1c 0a 01 01 03 04 04 00 00 00 03 11 00 57 56 51 50 53 52 5d 5c 5f 5e 59 58 5b 5a 55 54

- No.: 1313
- Timestamp: 20:28:46:894_0
- RFN: 2261
- Chip: 13312
- Event: Receive
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_CNF
- Source: ts_SS_DownloadSecurityKey:lt_DownloadKeyCRLC LINE 2
- Message Structure:
CRLC_SecurityMode_Config_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1320
- Timestamp: 20:28:46:897_0
- RFN: 2261
- Chip: 25856
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 1
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
. (IntegerType)count_I_LSB_UL = -
. (IntegerType)count_I_LSB_DL = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 00 02 01 00 02 01 00

- No.: 1321
- Timestamp: 20:28:46:899_0
- RFN: 2261
- Chip: 33280
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 2
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 00 02 01 00

- No.: 1322
- Timestamp: 20:28:46:901_0
- RFN: 2262
- Chip: 2048
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 3
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. (IntegerType)count_I_LSB_UL = -
. (IntegerType)count_I_LSB_DL = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 01 02 01 00

- No.: 1323
- Timestamp: 20:28:46:902_0
- RFN: 2262
- Chip: 8960
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 4
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 1324
- Timestamp: 20:28:46:904_0
- RFN: 2262
- Chip: 16128
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 5
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. (IntegerType)count_I_LSB_UL = -
. (IntegerType)count_I_LSB_DL = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 02 02 01 00

- No.: 1325
- Timestamp: 20:28:46:906_0
- RFN: 2262
- Chip: 24064
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 6
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 1326
- Timestamp: 20:28:46:908_0
- RFN: 2262
- Chip: 30976
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 7
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
. (IntegerType)count_I_LSB_UL = -
. (IntegerType)count_I_LSB_DL = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 03 02 01 00

- No.: 1327
- Timestamp: 20:28:46:910_0
- RFN: 2262
- Chip: 37888
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 8
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 1328
- Timestamp: 20:28:46:912_0
- RFN: 2263
- Chip: 6912
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 9
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
. (IntegerType)count_I_LSB_UL = -
. (IntegerType)count_I_LSB_DL = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 04 02 01 00

- No.: 1329
- Timestamp: 20:28:46:914_0
- RFN: 2263
- Chip: 13824
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 10
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 1333
- Timestamp: 20:28:46:916_0
- RFN: 2263
- Chip: 24832
- Event: Send
- PCO: CRLC
- Message: CRLC_Integrity_Activate_REQ
- Source: ts_CRLC_DL_Integrity LINE 1
- Message Structure:
CRLC_Integrity_Activate_REQ
. (IntegerType)cellId = -1
. (CN_DomainIdentity)cn_DomainIdentity = 1
. IntegrityActivationInfo
. . IntegrityProtectionModeInfo
. . . IntegrityProtectionModeCommand
. . . . startIntegrityProtection
. . . . . (BitStringType)integrityProtInitNumber[32] = "00000000000000000000000000000001"
. . . (IntegrityProtectionAlgorithm)integrityProtectionAlgorithm = 0
- Constraint:
ca_CRLC_DL_IntegrityActivateReq
- BinaryMessage:
30 15 02 01 ff 0a 01 01 30 0d 30 30 07 03 05 00 00 00 00 01 0a 01 00

- No.: 1334
- Timestamp: 20:28:46:918_0
- RFN: 2263
- Chip: 31488
- Event: Receive
- PCO: CRLC
- Message: CRLC_Integrity_Activate_CNF
- Source: ts_CRLC_DL_Integrity LINE 2
- Message Structure:
CRLC_Integrity_Activate_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_IntegrityActivateCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1341
- Timestamp: 20:28:46:922_0
- RFN: 2264
- Chip: 7680
- Event: Send
- PCO: CRLC
- Message: CRLC_Integrity_Activate_REQ
- Source: ts_RB2_UL_IntegrityActivate LINE 1
- Message Structure:
CRLC_Integrity_Activate_REQ
. (IntegerType)cellId = -1
. (CN_DomainIdentity)cn_DomainIdentity = 1
. IntegrityActivationInfo
. . IntegrityProtActivationInfoList
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity = 2
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
- Constraint:
ca_CRLC_UL_IntegrityActivateReq
- BinaryMessage:
30 10 02 01 ff 0a 01 01 30 08 30 06 02 01 02 02 01 00

- No.: 1342
- Timestamp: 20:28:46:923_0
- RFN: 2264
- Chip: 13568
- Event: Receive
- PCO: CRLC
- Message: CRLC_Integrity_Activate_CNF
- Source: ts_RB2_UL_IntegrityActivate LINE 2
- Message Structure:
CRLC_Integrity_Activate_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_IntegrityActivateCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1348
- Timestamp: 20:28:46:930_0
- RFN: 2264
- Chip: 37632
- Event: Send
- PCO: AM
- Message: RLC_AM_DATA_REQ
- Source: ts_RRC_Security:lt_SendSecurityModeCommand LINE 7
- Message Structure:
RLC_AM_DATA_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. AmConfirmationRequest
. aM_message
. . DL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00000000000000000000000000000000"
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . DL_DCCH_MessageType
. . . . SecurityModeCommand
. . . . . r3
. . . . . . SecurityModeCommand_r3_IEs
. . . . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . . . SecurityCapability
. . . . . . . . (BitStringType)cipheringAlgorithmCap[16] = '0000000000000011'B
. . . . . . . . (BitStringType)integrityProtectionAlgorithmCap[16] = '0000000000000010'B
. . . . . . . CipheringModeInfo
. . . . . . . IntegrityProtectionModeInfo
. . . . . . . . IntegrityProtectionModeCommand
. . . . . . . . . startIntegrityProtection
. . . . . . . . . . (BitStringType)integrityProtInitNumber[32] = "00000000000000000000000000000001"
. . . . . . . . (IntegrityProtectionAlgorithm)integrityProtectionAlgorithm = 0
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity = 1
. . . . . . . InterRAT_UE_SecurityCapList
. . . . . . laterNonCriticalExtensions
- Constraint:
cas_RRC_SecModeCmd
- BinaryMessage:
30 17 02 01 ff 02 01 02 05 00 80 00 00 00 04 04 00 01 80 01 40 00 00 00 30

- No.: 1354
- Timestamp: 20:28:47:073_0
- RFN: 2279
- Chip: 12800
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_IND
- Source: ts_RRC_Security:lt_StartSecurity_UE LINE 8
- Message Structure:
RLC_AM_DATA_IND
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. IntegrityResult
. . (IntegrityStatus)integrityUsed = 0
. aM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "10000001100000001110110111011101"
. . . . (IntegerType)rrc_MessageSequenceNumber = 1
. . . UL_DCCH_MessageType
. . . . SecurityModeComplete
. . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . IntegrityProtActivationInfo
. . . . . . RRC_MessageSequenceNumberList
. . . . . . . (IntegerType)_elem = 0
. . . . . . . (IntegerType)_elem = 0
. . . . . . . (IntegerType)_elem = 0
. . . . . . . (IntegerType)_elem = 0
. . . . . . . (IntegerType)_elem = 0
. . . . . laterNonCriticalExtensions
. . . . . . (BitStringType)securityModeComplete_r3_add_ext = 0
. . . . . . nonCriticalExtensions
- Constraint:
car_RRC_SecModeCmpl
- BinaryMessage:
30 12 02 01 ff 02 01 02 0a 01 00 c0 c0 76 ee 8d 21 00 00 00

- No.: 1355
- Timestamp: 20:28:47:074_0
- RFN: 2279
- Chip: 16896
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_Security:lt_StartSecurity_UE LINE 8
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1357
- Timestamp: 20:28:47:078_0
- RFN: 2279
- Chip: 32000
- Event: Send
- PCO: CRLC
- Message: CRLC_Integrity_Activate_REQ
- Source: ts_CRLC_UL_Integrity LINE 1
- Message Structure:
CRLC_Integrity_Activate_REQ
. (IntegerType)cellId = -1
. (CN_DomainIdentity)cn_DomainIdentity = 1
. IntegrityActivationInfo
. . IntegrityProtActivationInfoList
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity = 0
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity = 1
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity = 3
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity = 4
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
- Constraint:
ca_CRLC_UL_IntegrityActivateReq
- BinaryMessage:
30 28 02 01 ff 0a 01 01 30 20 30 06 02 01 00 02 01 00 30 06 02 01 01 02 01 00 30 06 02 01 03 02 01 00 30 06 02 01 04 02 01 00

- No.: 1358
- Timestamp: 20:28:47:080_0
- RFN: 2280
- Chip: 1024
- Event: Receive
- PCO: CRLC
- Message: CRLC_Integrity_Activate_CNF
- Source: ts_CRLC_UL_Integrity LINE 2
- Message Structure:
CRLC_Integrity_Activate_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_IntegrityActivateCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1368
- Timestamp: 20:28:47:087_0
- RFN: 2280
- Chip: 30720
- Event: Send
- PCO: Dc
- Message: RRC_DataReq
- Source: ts_GMM_IdleUpdated:lt_AttachAccept LINE 12
- Message Structure:
RRC_DataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[-1] = -
. (SapId)sapId[1] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. ATTACHACCEPT
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)gMMProtocolDiscriminator[4] = '1000'B
. . (MsgType)msgType[8] = '00000010'B
. . ForceToStandby
. . . (B1)spare[1] = '0'B
. . . (B3)value[3] = '000'B
. . AttachResult
. . . (B1)spare[1] = '0'B
. . . (B3)result[3] = '001'B
. . GPRS_Timer_v
. . . (B3)unit[3] = '111'B
. . . (B5)value[5] = '00000'B
. . (B4)spare[4] = '0000'B
. . RadioPriority_v
. . . (B1)spare[1] = '0'B
. . . (B3)value[3] = '100'B
. . RAI_v
. . . (OctetStringType)plmn[3] = '00F110'O
. . . (OctetStringType)lac[2] = '0001'O
. . . (OctetStringType)rac[1] = '05'O
. . PTMSI_Signature
. . . (IEI8)iei[8] = '00011001'B
. . . (OctetStringType)value[3] = 'AB1234'O
. . GPRS_Timer
. . GMM_MS_IdentityPTMSI
. . . (IEI8)iei[8] = '00011000'B
. . . (Length)iel[1] = '05'O
. . . (B4)iDigit1[4] = '1111'B
. . . (B1)oddEvenInd[1] = '0'B
. . . (B3)typeOfId[3] = '100'B
. . . (OctetStringType)otherDigits[-1] = '12345678'O
. . GMM_MS_Identity
. . GMM_Cause
. . GPRS_Timer
. . CellNotification
. . PLMN_List
- Constraint:
ca_PS_DataReq
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 08 02 01 e0 04 00 f1 10 00 01 05 19 ab 12 34 18 05 f4 12 34 56 78

- No.: 1372
- Timestamp: 20:28:47:221_0
- RFN: 2294
- Chip: 5632
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_GMM_IdleUpdated:lt_AttachAccept LINE 13
- Message Structure:
RRC_DataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. (START_Value)start[0] = -
. ATTACHCOMPLETE
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)gMMProtocolDiscriminator[4] = '1000'B
. . (MsgType)msgType[8] = '00000011'B
- Constraint:
car_PS_UplinkDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 08 03

- No.: 1383
- Timestamp: 20:28:47:225_0
- RFN: 2294
- Chip: 18688
- Event: Start Timer
- Source: ts_RRC_Delay LINE 1
- Message Structure:
no details available
- Constraint:
t_Dly (1000 Ms)
- BinaryMessage:

- No.: 1387
- Timestamp: 20:28:48:215_0
- RFN: 2393
- Chip: 20224
- Event: Timeout
- Source: ts_RRC_Delay LINE 2
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 1392
- Timestamp: 20:28:48:220_0
- RFN: 2394
- Chip: 2560
- Event: Send
- PCO: UM
- Message: RLC_UM_DATA_REQ
- Source: ts_RRC_ConnRel:lt_Send_RRC_ConnectionRelease LINE 3
- Message Structure:
RLC_UM_DATA_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. uM_message
. . DL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00000000000000000000000000000000"
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . DL_DCCH_MessageType
. . . . RRCConnectionRelease
. . . . . r3
. . . . . . RRCConnectionRelease_r3_IEs
. . . . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . . . (IntegerType)n_308 = 1
. . . . . . . (ReleaseCause)releaseCause = 0
. . . . . . . Rplmn_Information
. . . . . . laterNonCriticalExtensions
. (BooleanType)specialLI = FALSE
- Constraint:
cas_RRC_ConnRelDCCH
- BinaryMessage:
30 10 02 01 ff 02 01 01 80 00 00 00 03 c8 00 01 01 00

- No.: 1396
- Timestamp: 20:28:48:352_0
- RFN: 2407
- Chip: 8704
- Event: Receive
- PCO: UM
- Message: RLC_UM_DATA_IND
- Source: ts_RRC_ConnRel:lt_Send_RRC_ConnectionRelease LINE 4
- Message Structure:
RLC_UM_DATA_IND
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. IntegrityResult
. uM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "10101101101011101001000000111001"
. . . . (IntegerType)rrc_MessageSequenceNumber = 1
. . . UL_DCCH_MessageType
. . . . RRCConnectionReleaseComplete
. . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . FailureCauseWithProtErr
. . . . . laterNonCriticalExtensions
. . . . . . (BitStringType)rrcConnectionReleaseComplete_r3_add_ext = 0
. . . . . . nonCriticalExtensions
- Constraint:
car_RRC_ConnRelCmplUM
- BinaryMessage:
30 0c 02 01 ff 02 01 01 d6 d7 48 1c 8c 40

- No.: 1397
- Timestamp: 20:28:48:354_0
- RFN: 2407
- Chip: 12288
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ConnRel:lt_Send_RRC_ConnectionRelease LINE 4
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1400
- Timestamp: 20:28:48:355_0
- RFN: 2407
- Chip: 17152
- Event: Start Timer
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 1
- Message Structure:
no details available
- Constraint:
t_Dly (5000 Ms)
- BinaryMessage:

- No.: 1404
- Timestamp: 20:28:48:512_0
- RFN: 2423
- Chip: 7424
- Event: Receive
- PCO: UM
- Message: RLC_UM_DATA_IND
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 4
- Message Structure:
RLC_UM_DATA_IND
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. IntegrityResult
. uM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00011100010101000111110101101001"
. . . . (IntegerType)rrc_MessageSequenceNumber = 2
. . . UL_DCCH_MessageType
. . . . RRCConnectionReleaseComplete
. . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . FailureCauseWithProtErr
. . . . . laterNonCriticalExtensions
. . . . . . (BitStringType)rrcConnectionReleaseComplete_r3_add_ext = 0
. . . . . . nonCriticalExtensions
- Constraint:
car_RRC_ConnRelCmplUM
- BinaryMessage:
30 0c 02 01 ff 02 01 01 8e 2a 3e b4 94 40

- No.: 1405
- Timestamp: 20:28:48:513_0
- RFN: 2423
- Chip: 11008
- Event: Cancel Timer
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 4
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 1406
- Timestamp: 20:28:48:513_1
- RFN: 2423
- Chip: 12032
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 4
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1412
- Timestamp: 20:28:48:517_0
- RFN: 2423
- Chip: 25856
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 01 0a 01 00 05 00

- No.: 1416
- Timestamp: 20:28:48:524_0
- RFN: 2424
- Chip: 17152
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 1419
- Timestamp: 20:28:48:527_0
- RFN: 2424
- Chip: 28160
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 02 0a 01 00 05 00

- No.: 1423
- Timestamp: 20:28:48:534_0
- RFN: 2425
- Chip: 17920
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 1426
- Timestamp: 20:28:48:537_0
- RFN: 2425
- Chip: 28672
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 03 0a 01 00 05 00

- No.: 1430
- Timestamp: 20:28:48:548_0
- RFN: 2426
- Chip: 30464
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 1433
- Timestamp: 20:28:48:551_0
- RFN: 2427
- Chip: 6144
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 04 0a 01 00 05 00

- No.: 1437
- Timestamp: 20:28:48:561_0
- RFN: 2428
- Chip: 5888
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 1440
- Timestamp: 20:28:48:569_0
- RFN: 2428
- Chip: 34560
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 136
. . . . . UL_RLC_Mode
. . . . . . UL_UM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (NoExplicitDiscard)timerBasedNoExplicit = 9
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = 1
. . . . (IntegerType)dLlogicalChannelIdentity = 1
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_UM_Info
- BinaryMessage:
30 22 02 01 ff 02 01 01 0a 01 00 30 17 30 0d 05 00 30 09 02 02 00 88 30 03 0a 01 09 30 06 02 01 01 02 01 01

- No.: 1444
- Timestamp: 20:28:48:580_0
- RFN: 2430
- Chip: 0
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 1445
- Timestamp: 20:28:48:588_0
- RFN: 2430
- Chip: 31488
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 3
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . (TimerEPC)timerEPC = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . (TimerRST)timerRST = 9
. . . . . . . (MaxRST)max_RST = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = 2
. . . . (IntegerType)dLlogicalChannelIdentity = 2
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 02 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 27 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 02 02 01 02

- No.: 1449
- Timestamp: 20:28:48:607_0
- RFN: 2432
- Chip: 29440
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 4
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 1450
- Timestamp: 20:28:48:616_0
- RFN: 2433
- Chip: 24320
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 5
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . (TimerEPC)timerEPC = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . (TimerRST)timerRST = 9
. . . . . . . (MaxRST)max_RST = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = 3
. . . . (IntegerType)dLlogicalChannelIdentity = 3
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 03 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 27 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 03 02 01 03

- No.: 1454
- Timestamp: 20:28:48:633_0
- RFN: 2435
- Chip: 13312
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 6
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 1455
- Timestamp: 20:28:48:642_0
- RFN: 2436
- Chip: 8704
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 7
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . (TimerEPC)timerEPC = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . (TimerRST)timerRST = 9
. . . . . . . (MaxRST)max_RST = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = 4
. . . . (IntegerType)dLlogicalChannelIdentity = 4
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 04 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 27 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 04 02 01 04

- No.: 1459
- Timestamp: 20:28:48:663_0
- RFN: 2438
- Chip: 13312
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 8
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 1501
- Timestamp: 20:28:48:676_2
- RFN: 2439
- Chip: 23040
- Event: Start Timer
- Source: ts_RRC_Delay LINE 1
- Message Structure:
no details available
- Constraint:
t_Dly (5000 Ms)
- BinaryMessage:

- No.: 1503
- Timestamp: 20:28:48:679_0
- RFN: 2439
- Chip: 33536
- Event: Receive
- PCO: CPHY
- Message: CPHY_Out_of_Sync_IND
- Source: RRC_Def1 LINE 15
- Message Structure:
CPHY_Out_of_Sync_IND
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_OutOfSyncInd
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 1504
- Timestamp: 20:28:48:680_0
- RFN: 2439
- Chip: 35584
- Event: Cancel Timer
- Source: RRC_Def1 LINE 15
- Message Structure:
no details available
- Constraint:
t_T312
- BinaryMessage:

- No.: 1505
- Timestamp: 20:28:48:680_1
- RFN: 2439
- Chip: 37632
- Event: Default
- Source: RRC_Def1 LINE 0
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1506
- Timestamp: 20:28:48:680_2
- RFN: 2440
- Chip: 0
- Event: Default
- Source: ts_RRC_Delay LINE 2
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1511
- Timestamp: 20:28:53:666_0
- RFN: 2938
- Chip: 26112
- Event: Timeout
- Source: ts_RRC_Delay LINE 2
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 1524
- Timestamp: 20:28:53:679_0
- RFN: 2939
- Chip: 37376
- Event: Send
- PCO: CMAC
- Message: CMAC_PAGING_Config_REQ
- Source: ts_CMAC_Pag1_Cfg LINE 4
- Message Structure:
CMAC_PAGING_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 5
. (RatType)ratType = 0
. CmacPagingConfigReq
. . pI_BitMapInfo
. . . (BitStringType)e18[18] = '010000000000000000'B
. . (IntegerType)dRX_CycleLength = 7
. . IMSI_GSM_MAP
. . . (IntegerType)_elem = 0
. . . (IntegerType)_elem = 0
. . . (IntegerType)_elem = 1
. . . (IntegerType)_elem = 0
. . . (IntegerType)_elem = 1
. . . (IntegerType)_elem = 0
. . . (IntegerType)_elem = 1
. . . (IntegerType)_elem = 2
. . . (IntegerType)_elem = 3
. . . (IntegerType)_elem = 4
. . . (IntegerType)_elem = 5
. . . (IntegerType)_elem = 6
. . . (IntegerType)_elem = 0
. . . (IntegerType)_elem = 6
. . . (IntegerType)_elem = 3
. . (BooleanType)t_pich_T_sccpch = FALSE
- Constraint:
ca_CMAC_PagingCfgReq
- BinaryMessage:
30 46 02 01 00 02 01 05 0a 01 00 30 3b 03 04 06 40 00 00 02 01 07 30 2d 02 01 00 02 01 00 02 01 01 02 01 00 02 01 01 02 01 00 02 01 01 02 01 02 02 01 03 02 01 04 02 01 05 02 01 06 02 01 00 02 01 06 02 01 03 01 01 00

- No.: 1528
- Timestamp: 20:28:53:688_0
- RFN: 2940
- Chip: 27904
- Event: Receive
- PCO: CMAC
- Message: CMAC_PAGING_Config_CNF
- Source: ts_CMAC_Pag1_Cfg LINE 5
- Message Structure:
CMAC_PAGING_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 5
- Constraint:
ca_CMAC_PagingCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 05

- No.: 1530
- Timestamp: 20:28:53:697_0
- RFN: 2941
- Chip: 24576
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_RRC_ConnEst_DCH_MT_PTMSI LINE 5
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -2
. tM_message
. . PCCH_Message
. . . PCCH_MessageType
. . . . PagingType1
. . . . . PagingRecordList
. . . . . . PagingRecord
. . . . . . . cn_Identity
. . . . . . . . (PagingCause)pagingCause = 2
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = 1
. . . . . . . . CN_PagedUE_Identity
. . . . . . . . . (BitStringType)p_TMSI_GSM_MAP[32] = "00010010001101000101011001111000"
. . . . . BCCH_ModificationInfo
. . . . . laterNonCriticalExtensions
- Constraint:
cas_PagingType1
- BinaryMessage:
30 0c 02 01 00 02 01 fe 40 54 24 68 ac f0

- No.: 1534
- Timestamp: 20:28:54:632_0
- RFN: 3035
- Chip: 6144
- Event: Receive
- PCO: TM
- Message: RLC_TR_DATA_IND
- Source: ts_RRC_ConnEst_DCH_MT_PTMSI LINE 6
- Message Structure:
RLC_TR_DATA_IND
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
. tM_message
. . UL_CCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode = 0
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . UL_CCCH_MessageType
. . . . RRCConnectionRequest
. . . . . InitialUE_Identity
. . . . . . TMSI_and_LAI_GSM_MAP
. . . . . . . (BitStringType)tmsi[32] = "00010010001101000101011001111000"
. . . . . . . LAI
. . . . . . . . PLMN_Identity
. . . . . . . . . MCC
. . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . (IntegerType)_elem = 1
. . . . . . . . . MNC
. . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . (IntegerType)_elem = 1
. . . . . . . . (BitStringType)lac[16] = '0000000000000001'B
. . . . . (EstablishmentCause)establishmentCause = 7
. . . . . (ProtocolErrorIndicator)protocolErrorIndicator = 0
. . . . . MeasuredResultsOnRACH
. . . . . . currentCell
. . . . . . . modeSpecificInfo
. . . . . . . . fdd
. . . . . . . . . measurementQuantity
. . . . . . . . . . (IntegerType)cpich_Ec_N0 = 0
. . . . . v3d0NonCriticalExtensions
. . . . . . RRCConnectionRequest_v3d0ext_IEs
. . . . . . . (BitStringType)uESpecificBehaviourInformation1idle = 0
. . . . . . nonCriticalExtensions
- Constraint:
car_RRC_ConnReq
- BinaryMessage:
30 11 02 01 00 02 01 00 21 12 34 56 78 00 10 08 00 09 c0

- No.: 1535
- Timestamp: 20:28:54:693_0
- RFN: 3041
- Chip: 11008
- Event: Send
- PCO: UM
- Message: RLC_UM_DATA_REQ
- Source: ts_RRC_ConnEst_DCH_MT_PTMSI LINE 7
- Message Structure:
RLC_UM_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
. uM_message
. . DL_CCCH_Message
. . . IntegrityCheckInfo
. . . DL_CCCH_MessageType
. . . . RRCConnectionSetup
. . . . . r3
. . . . . . RRCConnectionSetup_r3_IEs
. . . . . . . InitialUE_Identity
. . . . . . . . TMSI_and_LAI_GSM_MAP
. . . . . . . . . (BitStringType)tmsi[32] = "00010010001101000101011001111000"
. . . . . . . . . LAI
. . . . . . . . . . PLMN_Identity
. . . . . . . . . . . MCC
. . . . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . . . (IntegerType)_elem = 1
. . . . . . . . . . . MNC
. . . . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . . . (IntegerType)_elem = 1
. . . . . . . . . . (BitStringType)lac[16] = '0000000000000001'B
. . . . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . . . (IntegerType)activationTime = -
. . . . . . . U_RNTI
. . . . . . . . (BitStringType)srnc_Identity[12] = "000000000001"
. . . . . . . . (BitStringType)s_RNTI[20] = "00000000000000000001"
. . . . . . . (BitStringType)new_c_RNTI[16] = -
. . . . . . . (RRC_StateIndicator)rrc_StateIndicator = 0
. . . . . . . (IntegerType)utran_DRX_CycleLengthCoeff = 9
. . . . . . . CapabilityUpdateRequirement
. . . . . . . . (BooleanType)ue_RadioCapabilityFDDUpdateRequirement = TRUE
. . . . . . . . (BooleanType)ue_RadioCapabilityTDDUpdateRequirement = FALSE
. . . . . . . . SystemSpecificCapUpdateReqList
. . . . . . . . . (SystemSpecificCapUpdateReq)_elem = 0
. . . . . . . SRB_InformationSetupList2
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_UM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 1
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 1
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . . . . . . . (TimerRST)timerRST = 9
. . . . . . . . . . . . . (MaxRST)max_RST = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 2
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 2
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . . . . . . . (TimerRST)timerRST = 9
. . . . . . . . . . . . . (MaxRST)max_RST = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 3
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 3
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . . . . . . . (TimerRST)timerRST = 9
. . . . . . . . . . . . . (MaxRST)max_RST = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 4
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 4
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . UL_CommonTransChInfo
. . . . . . . . TFC_Subset
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . TFCS
. . . . . . . . . . . ExplicitTFCS_Configuration
. . . . . . . . . . . . TFCS_ReconfAdd
. . . . . . . . . . . . . ctfcSize
. . . . . . . . . . . . . . ctfc2Bit
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . . . . . . . (IntegerType)ctfc2 = 0
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . . . . . . . (IntegerType)ctfc2 = 1
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 11
. . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . UL_AddReconfTransChInfoList
. . . . . . . . UL_AddReconfTransChInformation
. . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType = 0
. . . . . . . . . (IntegerType)transportChannelIdentity = 5
. . . . . . . . . TransportFormatSet
. . . . . . . . . . DedicatedTransChTFS
. . . . . . . . . . . tti
. . . . . . . . . . . . DedicatedDynamicTF_InfoList
. . . . . . . . . . . . . DedicatedDynamicTF_Info
. . . . . . . . . . . . . . rlc_Size
. . . . . . . . . . . . . . . BitModeRLC_SizeInfo
. . . . . . . . . . . . . . . . sizeType2
. . . . . . . . . . . . . . . . . (IntegerType)part1 = 2
. . . . . . . . . . . . . . . . . (IntegerType)part2 = -
. . . . . . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . LogicalChannelList
. . . . . . . . . . . SemistaticTF_Information
. . . . . . . . . . . . ChannelCodingType
. . . . . . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . . . . . (IntegerType)rateMatchingAttribute = 192
. . . . . . . . . . . . (CRC_Size)crc_Size = 3
. . . . . . . DL_CommonTransChInfo
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . dl_Parameters
. . . . . . . DL_AddReconfTransChInfoList
. . . . . . . . DL_AddReconfTransChInformation
. . . . . . . . . (DL_TrCH_Type)dl_TransportChannelType = 0
. . . . . . . . . (IntegerType)dl_transportChannelIdentity = 10
. . . . . . . . . tfs_SignallingMode
. . . . . . . . . . UL_TransportChannelIdentity
. . . . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType = 0
. . . . . . . . . . . (IntegerType)ul_TransportChannelIdentity = 5
. . . . . . . . . QualityTarget
. . . . . . . . . . (IntegerType)bler_QualityValue = -20
. . . . . . . . . TM_SignallingInfo
. . . . . . . FrequencyInfo
. . . . . . . (IntegerType)maxAllowedUL_TX_Power = -
. . . . . . . UL_ChannelRequirement
. . . . . . . . UL_DPCH_Info
. . . . . . . . . UL_DPCH_PowerControlInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (IntegerType)dpcch_PowerOffset = -40
. . . . . . . . . . . (IntegerType)pc_Preamble = 1
. . . . . . . . . . . (IntegerType)sRB_delay = 7
. . . . . . . . . . . PowerControlAlgorithm
. . . . . . . . . . . . (IntegerType)algorithm1 = 1
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (ScramblingCodeType)scramblingCodeType = 1
. . . . . . . . . . . (IntegerType)scramblingCode = 0
. . . . . . . . . . . (IntegerType)numberOfDPDCH = -
. . . . . . . . . . . (SpreadingFactor)spreadingFactor = 4
. . . . . . . . . . . (BooleanType)tfci_Existence = TRUE
. . . . . . . . . . . (IntegerType)numberOfFBI_Bits = -
. . . . . . . . . . . (PuncturingLimit)puncturingLimit = 15
. . . . . . . DL_CommonInformation
. . . . . . . . DL_DPCH_InfoCommon
. . . . . . . . . cfnHandling
. . . . . . . . . . initialise
. . . . . . . . . . . (IntegerType)cfntargetsfnframeoffset = -
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . DL_DPCH_PowerControlInfo
. . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . (DPC_Mode)dpc_Mode = 0
. . . . . . . . . . . (IntegerType)powerOffsetPilot_pdpdch = 0
. . . . . . . . . . . Dl_rate_matching_restriction
. . . . . . . . . . . SF512_AndPilot
. . . . . . . . . . . . (PilotBits128)sfd128 = 0
. . . . . . . . . . . (PositionFixedOrFlexible)positionFixedOrFlexible = 0
. . . . . . . . . . . (BooleanType)tfci_Existence = FALSE
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . (IntegerType)defaultDPCH_OffsetValue = 0
. . . . . . . . . . DPCH_CompressedModeInfo
. . . . . . . . . . (TX_DiversityMode)tx_DiversityMode = 0
. . . . . . . . . . SSDT_Information
. . . . . . . DL_InformationPerRL_List
. . . . . . . . DL_InformationPerRL
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . PrimaryCPICH_Info
. . . . . . . . . . . . (IntegerType)primaryScramblingCode = 100
. . . . . . . . . . . PDSCH_SHO_DCH_Info
. . . . . . . . . . . PDSCH_CodeMapping
. . . . . . . . . DL_DPCH_InfoPerRL
. . . . . . . . . . fdd
. . . . . . . . . . . (PCPICH_UsageForChannelEst)pCPICH_UsageForChannelEst = 0
. . . . . . . . . . . (IntegerType)dpch_FrameOffset = 0
. . . . . . . . . . . SecondaryCPICH_Info
. . . . . . . . . . . DL_ChannelisationCodeList
. . . . . . . . . . . . DL_ChannelisationCode
. . . . . . . . . . . . . (IntegerType)secondaryScramblingCode = 1
. . . . . . . . . . . . . SF512_AndCodeNumber
. . . . . . . . . . . . . . (IntegerType)sf128 = 0
. . . . . . . . . . . . . (ScramblingCodeChange)scramblingCodeChange = 1
. . . . . . . . . . . (IntegerType)tpc_CombinationIndex = 0
. . . . . . . . . . . (SSDT_CellIdentity)ssdt_CellIdentity = -
. . . . . . . . . . . (ClosedLoopTimingAdjMode)closedLoopTimingAdjMode = -
. . . . . . . . . SCCPCH_InfoForFACH
. . . . . . laterNonCriticalExtensions
. (BooleanType)specialLI = TRUE
- Constraint:
cas_RRC_ConnSetup
- BinaryMessage:
30 78 02 01 00 02 01 00 30 e7 22 46 8a cf 00 02 01 00 01 00 04 00 00 4d 82 69 3a 10 10 89 0d 42 00 02 81 9e 8e 46 c9 ce 7c 9c 4e 74 20 a5 12 3a 8c 00 15 13 3d 1c 8d 93 9c f9 38 9c e8 42 52 24 b5 28 00 4a 46 7a 39 1b 27 39 f2 71 39 d0 86 b4 49 ea 70 00 d4 c8 00 06 25 2b f0 02 00 08 82 23 bf 66 08 98 95 a5 47 a2 00 00 01 3f 90 0a 14 00 02 06 40 00 0c 28 08 01 01 ff

- No.: 1543
- Timestamp: 20:28:54:734_1
- RFN: 3045
- Chip: 15104
- Event: Start Timer
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 3
- Message Structure:
no details available
- Constraint:
t_WaitMS (13500 Ms)
- BinaryMessage:

- No.: 1548
- Timestamp: 20:28:54:959_0
- RFN: 3067
- Chip: 34304
- Event: Receive
- PCO: CPHY
- Message: CPHY_Sync_IND
- Source: RRC_Def1 LINE 13
- Message Structure:
CPHY_Sync_IND
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_SyncInd
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 1549
- Timestamp: 20:28:54:960_0
- RFN: 3067
- Chip: 36096
- Event: Cancel Timer
- Source: RRC_Def1 LINE 13
- Message Structure:
no details available
- Constraint:
t_T312
- BinaryMessage:

- No.: 1550
- Timestamp: 20:28:54:960_1
- RFN: 3067
- Chip: 37888
- Event: Default
- Source: RRC_Def1 LINE 0
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1551
- Timestamp: 20:28:54:960_2
- RFN: 3068
- Chip: 256
- Event: Default
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1556
- Timestamp: 20:28:55:075_0
- RFN: 3079
- Chip: 20480
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_IND
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
RLC_AM_DATA_IND
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. IntegrityResult
. . (IntegrityStatus)integrityUsed = 0
. aM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode = 0
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . UL_DCCH_MessageType
. . . . RRCConnectionSetupComplete
. . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . STARTList
. . . . . . STARTSingle
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity = 1
. . . . . . . (BitStringType)start_Value[20] = "00000000000000000010"
. . . . . . STARTSingle
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity = 0
. . . . . . . (BitStringType)start_Value[20] = "00000000000000000010"
. . . . . UE_RadioAccessCapability
. . . . . . (AccessStratumReleaseIndicator)accessStratumReleaseIndicator = 0
. . . . . . PDCP_Capability
. . . . . . . (BooleanType)losslessSRNS_RelocationSupport = FALSE
. . . . . . . supportForRfc2507
. . . . . . RLC_Capability
. . . . . . . (TotalRLC_AM_BufferSize)totalRLC_AM_BufferSize = 2
. . . . . . . (MaximumRLC_WindowSize)maximumRLC_WindowSize = 0
. . . . . . . (MaximumAM_EntityNumberRLC_Cap)maximumAM_EntityNumber = 3
. . . . . . TransportChannelCapability
. . . . . . . DL_TransChCapability
. . . . . . . . (MaxNoBits)maxNoBitsReceived = 4
. . . . . . . . (MaxNoBits)maxConvCodeBitsReceived = 1
. . . . . . . . TurboSupport
. . . . . . . . . (MaxNoBits)supported = 4
. . . . . . . . (MaxSimultaneousTransChsDL)maxSimultaneousTransChs = 1
. . . . . . . . (IntegerType)maxSimultaneousCCTrCH_Count = 1
. . . . . . . . (MaxTransportBlocksDL)maxReceivedTransportBlocks = 2
. . . . . . . . (MaxNumberOfTFC_DL)maxNumberOfTFC = 4
. . . . . . . . (MaxNumberOfTF)maxNumberOfTF = 1
. . . . . . . UL_TransChCapability
. . . . . . . . (MaxNoBits)maxNoBitsTransmitted = 3
. . . . . . . . (MaxNoBits)maxConvCodeBitsTransmitted = 1
. . . . . . . . TurboSupport
. . . . . . . . . (MaxNoBits)supported = 3
. . . . . . . . (MaxSimultaneousTransChsUL)maxSimultaneousTransChs = 2
. . . . . . . . modeSpecificInfo
. . . . . . . . (MaxTransportBlocksUL)maxTransmittedBlocks = 2
. . . . . . . . (MaxNumberOfTFC_UL)maxNumberOfTFC = 3
. . . . . . . . (MaxNumberOfTF)maxNumberOfTF = 0
. . . . . . RF_Capability
. . . . . . . fddRF_Capability
. . . . . . . . (IntegerType)ue_PowerClass = 4
. . . . . . . . (TxRxFrequencySeparation)txRxFrequencySeparation = 0
. . . . . . . tddRF_Capability
. . . . . . . . (IntegerType)ue_PowerClass = 0
. . . . . . . . (RadioFrequencyBandTDDList)radioFrequencyTDDBandList = 0
. . . . . . . . (ChipRateCapability)chipRateCapability = 0
. . . . . . PhysicalChannelCapability
. . . . . . . fddPhysChCapability
. . . . . . . . DL_PhysChCapabilityFDD
. . . . . . . . . (IntegerType)maxNoDPCH_PDSCH_Codes = 3
. . . . . . . . . (MaxNoPhysChBitsReceived)maxNoPhysChBitsReceived = 6
. . . . . . . . . (BooleanType)supportForSF_512 = FALSE
. . . . . . . . . (BooleanType)supportOfPDSCH = FALSE
. . . . . . . . . SimultaneousSCCPCH_DPCH_Reception
. . . . . . . . UL_PhysChCapabilityFDD
. . . . . . . . . (MaxNoDPDCH_BitsTransmitted)maxNoDPDCH_BitsTransmitted = 2
. . . . . . . . . (BooleanType)supportOfPCPCH = FALSE
. . . . . . . tddPhysChCapability
. . . . . . . . DL_PhysChCapabilityTDD
. . . . . . . . . (IntegerType)maxTS_PerFrame = 0
. . . . . . . . . (IntegerType)maxPhysChPerFrame = 0
. . . . . . . . . (MinimumSF_DL)minimumSF = 0
. . . . . . . . . (BooleanType)supportOfPDSCH = FALSE
. . . . . . . . . (IntegerType)maxPhysChPerTS = 0
. . . . . . . . UL_PhysChCapabilityTDD
. . . . . . . . . (IntegerType)maxTS_PerFrame = 0
. . . . . . . . . (MaxPhysChPerTimeslot)maxPhysChPerTimeslot = 0
. . . . . . . . . (MinimumSF_UL)minimumSF = 0
. . . . . . . . . (BooleanType)supportOfPUSCH = FALSE
. . . . . . UE_MultiModeRAT_Capability
. . . . . . . MultiRAT_Capability
. . . . . . . . (BooleanType)supportOfGSM = TRUE
. . . . . . . . (BooleanType)supportOfMulticarrier = FALSE
. . . . . . . (MultiModeCapability)multiModeCapability = 1
. . . . . . SecurityCapability
. . . . . . . (BitStringType)cipheringAlgorithmCap[16] = '0000000000000011'B
. . . . . . . (BitStringType)integrityProtectionAlgorithmCap[16] = '0000000000000010'B
. . . . . . UE_Positioning_Capability
. . . . . . . (BooleanType)standaloneLocMethodsSupported = FALSE
. . . . . . . (BooleanType)ue_BasedOTDOA_Supported = FALSE
. . . . . . . (NetworkAssistedGPS_Supported)networkAssistedGPS_Supported = 3
. . . . . . . (BooleanType)supportForUE_GPS_TimingOfCellFrames = FALSE
. . . . . . . (BooleanType)supportForIPDL = FALSE
. . . . . . MeasurementCapability
. . . . . . . CompressedModeMeasCapability
. . . . . . . . (BooleanType)fdd_Measurements = TRUE
. . . . . . . . (BooleanType)tdd_Measurements = FALSE
. . . . . . . . GSM_Measurements
. . . . . . . . . (BooleanType)gsm900 = TRUE
. . . . . . . . . (BooleanType)dcs1800 = TRUE
. . . . . . . . . (BooleanType)gsm1900 = FALSE
. . . . . . . . (BooleanType)multiCarrierMeasurements = FALSE
. . . . . . . CompressedModeMeasCapability
. . . . . . . . (BooleanType)fdd_Measurements = TRUE
. . . . . . . . (BooleanType)tdd_Measurements = FALSE
. . . . . . . . GSM_Measurements
. . . . . . . . . (BooleanType)gsm900 = TRUE
. . . . . . . . . (BooleanType)dcs1800 = TRUE
. . . . . . . . . (BooleanType)gsm1900 = FALSE
. . . . . . . . (BooleanType)multiCarrierMeasurements = FALSE
. . . . . v370NonCriticalExtensions
. . . . . . RRCConnectionSetupComplete_v370ext
. . . . . . . UE_RadioAccessCapability_v370ext
. . . . . . v380NonCriticalExtensions
. . . . . . . RRCConnectionSetupComplete_v380ext_IEs
. . . . . . . . UE_RadioAccessCapability_v380ext
. . . . . . . . . UE_PositioningCapabilityExt_v380
. . . . . . . . . . (BooleanType)rx_tx_TimeDifferenceType2Capable = FALSE
. . . . . . . . DL_PhysChCapabilityFDD_v380ext
. . . . . . . . . (SupportOfDedicatedPilotsForChEstimation)supportOfDedicatedPilotsForChEstimation = 0
. . . . . . . v3a0NonCriticalExtensions
. . . . . . . . RRCConnectionSetupComplete_v3a0ext_IEs
. . . . . . . . . UE_RadioAccessCapability_v3a0ext
. . . . . . . . . . UE_PositioningCapabilityExt_v3a0
. . . . . . . . . . . (UE_PositioningCapabilityExt_v3a0_list_0)validity_CellPCH_UraPCH = 0
. . . . . . . . laterNonCriticalExtensions
. . . . . . . . . (BitStringType)rrcConnectionSetupComplete_r3_add_ext = 0
. . . . . . . . . nonCriticalExtensions
- Constraint:
car_RRC_ConnSetupCmpl
- BinaryMessage:
30 27 02 01 ff 02 01 02 0a 05 01 00 00 00 00 4a 0c 00 00 80 00 05 11 a0 d1 04 84 c6 68 46 2c 93 02 48 00 18 00 11 8f 8f 80

- No.: 1557
- Timestamp: 20:28:55:086_0
- RFN: 3080
- Chip: 24320
- Event: Cancel Timer
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
t_WaitMS
- BinaryMessage:

- No.: 1558
- Timestamp: 20:28:55:086_1
- RFN: 3080
- Chip: 25344
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1572
- Timestamp: 20:28:55:094_0
- RFN: 3081
- Chip: 15104
- Event: Send
- PCO: CMAC
- Message: CMAC_SecurityMode_Config_REQ
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 1
- Message Structure:
CMAC_SecurityMode_Config_REQ
. (IntegerType)cellId = 0
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity = 1
. . (BitStringType)startValue[20] = "00000000000000000010"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = -
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CMAC_SecurityModeCfgReq
- BinaryMessage:
30 0e 02 01 00 30 09 0a 01 01 03 04 04 00 00 20

- No.: 1573
- Timestamp: 20:28:55:096_0
- RFN: 3081
- Chip: 22016
- Event: Receive
- PCO: CMAC
- Message: CMAC_SecurityMode_Config_CNF
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 2
- Message Structure:
CMAC_SecurityMode_Config_CNF
. (IntegerType)cellId = 0
- Constraint:
ca_CMAC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 00

- No.: 1574
- Timestamp: 20:28:55:098_0
- RFN: 3081
- Chip: 30720
- Event: Send
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_REQ
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 3
- Message Structure:
CRLC_SecurityMode_Config_REQ
. (IntegerType)cellId = -1
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity = 1
. . (BitStringType)startValue[20] = "00000000000000000010"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = -
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CRLC_SecurityModeCfgReq
- BinaryMessage:
30 0e 02 01 ff 30 09 0a 01 01 03 04 04 00 00 20

- No.: 1575
- Timestamp: 20:28:55:100_0
- RFN: 3081
- Chip: 37120
- Event: Receive
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_CNF
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 4
- Message Structure:
CRLC_SecurityMode_Config_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1589
- Timestamp: 20:28:55:105_0
- RFN: 3082
- Chip: 21760
- Event: Send
- PCO: CMAC
- Message: CMAC_SecurityMode_Config_REQ
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 1
- Message Structure:
CMAC_SecurityMode_Config_REQ
. (IntegerType)cellId = 0
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity = 0
. . (BitStringType)startValue[20] = "00000000000000000010"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = -
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CMAC_SecurityModeCfgReq
- BinaryMessage:
30 0e 02 01 00 30 09 0a 01 00 03 04 04 00 00 20

- No.: 1590
- Timestamp: 20:28:55:108_0
- RFN: 3082
- Chip: 29952
- Event: Receive
- PCO: CMAC
- Message: CMAC_SecurityMode_Config_CNF
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 2
- Message Structure:
CMAC_SecurityMode_Config_CNF
. (IntegerType)cellId = 0
- Constraint:
ca_CMAC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 00

- No.: 1591
- Timestamp: 20:28:55:110_0
- RFN: 3083
- Chip: 2048
- Event: Send
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_REQ
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 3
- Message Structure:
CRLC_SecurityMode_Config_REQ
. (IntegerType)cellId = -1
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity = 0
. . (BitStringType)startValue[20] = "00000000000000000010"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = -
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CRLC_SecurityModeCfgReq
- BinaryMessage:
30 0e 02 01 ff 30 09 0a 01 00 03 04 04 00 00 20

- No.: 1592
- Timestamp: 20:28:55:112_0
- RFN: 3083
- Chip: 9472
- Event: Receive
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_CNF
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 4
- Message Structure:
CRLC_SecurityMode_Config_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1613
- Timestamp: 20:28:55:123_0
- RFN: 3084
- Chip: 12800
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: pr_GenericSetupProcedures:lt_ReceiveResponseToPaging LINE 2
- Message Structure:
RRC_DataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. (START_Value)start[20] = '00000000000000000010'B
. SERVICEREQUEST
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)gMMProtocolDiscriminator[4] = '1000'B
. . (MsgType)msgType[8] = '00001100'B
. . ServiceType_v
. . . (B1)spare1[1] = '0'B
. . . (B3)type[3] = '010'B
. . CiphKeySeqNum
. . . (B1)spare1[1] = '0'B
. . . (KeySeq)keySeq[3] = '000'B
. . MS_Identity_lv
. . . (Length)iel[1] = '05'O
. . . (B4)iDigit1[4] = '1111'B
. . . (B1)oddEvenInd[1] = '0'B
. . . (B3)typeOfId[3] = '100'B
. . . (OctetStringType)otherDigits[4] = '12345678'O
. . PDP_ContextStatus
. . . (IEI8)iei[8] = '00110010'B
. . . (Length)iel[1] = '02'O
. . . (BitStringType)nSAPI[16] = '0000000000000000'B
- Constraint:
car_PS_InitDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 03 04 04 00 00 20 08 0c 20 05 f4 12 34 56 78 32 02 00 00

- No.: 1647
- Timestamp: 20:28:55:137_0
- RFN: 3085
- Chip: 28160
- Event: Send
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_REQ
- Source: ts_SS_DownloadSecurityKey:lt_DownloadKeyCRLC LINE 1
- Message Structure:
CRLC_SecurityMode_Config_REQ
. (IntegerType)cellId = -1
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity = 1
. . (BitStringType)startValue[20] = "00000000000000000010"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = '01010111010101100101000101010000010100110101001001011101010111000101111101011110010110010101100001011011010110100101010101010100'B
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CRLC_SecurityModeCfgReq
- BinaryMessage:
30 21 02 01 ff 30 1c 0a 01 01 03 04 04 00 00 20 03 11 00 57 56 51 50 53 52 5d 5c 5f 5e 59 58 5b 5a 55 54

- No.: 1648
- Timestamp: 20:28:55:139_0
- RFN: 3085
- Chip: 37120
- Event: Receive
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_CNF
- Source: ts_SS_DownloadSecurityKey:lt_DownloadKeyCRLC LINE 2
- Message Structure:
CRLC_SecurityMode_Config_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1655
- Timestamp: 20:28:55:143_0
- RFN: 3086
- Chip: 14080
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 1
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
. (IntegerType)count_I_LSB_UL = -
. (IntegerType)count_I_LSB_DL = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 00 02 01 00 02 01 00

- No.: 1656
- Timestamp: 20:28:55:145_0
- RFN: 3086
- Chip: 21504
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 2
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 00 02 01 00

- No.: 1657
- Timestamp: 20:28:55:147_0
- RFN: 3086
- Chip: 28672
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 3
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. (IntegerType)count_I_LSB_UL = -
. (IntegerType)count_I_LSB_DL = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 01 02 01 00

- No.: 1658
- Timestamp: 20:28:55:149_0
- RFN: 3086
- Chip: 35584
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 4
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 1659
- Timestamp: 20:28:55:151_0
- RFN: 3087
- Chip: 4096
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 5
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. (IntegerType)count_I_LSB_UL = -
. (IntegerType)count_I_LSB_DL = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 02 02 01 00

- No.: 1660
- Timestamp: 20:28:55:153_0
- RFN: 3087
- Chip: 11264
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 6
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 1661
- Timestamp: 20:28:55:154_0
- RFN: 3087
- Chip: 18176
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 7
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
. (IntegerType)count_I_LSB_UL = -
. (IntegerType)count_I_LSB_DL = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 03 02 01 00

- No.: 1662
- Timestamp: 20:28:55:156_0
- RFN: 3087
- Chip: 25600
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 8
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 1663
- Timestamp: 20:28:55:158_0
- RFN: 3087
- Chip: 32256
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 9
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
. (IntegerType)count_I_LSB_UL = -
. (IntegerType)count_I_LSB_DL = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 04 02 01 00

- No.: 1664
- Timestamp: 20:28:55:160_0
- RFN: 3088
- Chip: 1024
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 10
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 1668
- Timestamp: 20:28:55:163_0
- RFN: 3088
- Chip: 13824
- Event: Send
- PCO: CRLC
- Message: CRLC_Integrity_Activate_REQ
- Source: ts_CRLC_DL_Integrity LINE 1
- Message Structure:
CRLC_Integrity_Activate_REQ
. (IntegerType)cellId = -1
. (CN_DomainIdentity)cn_DomainIdentity = 1
. IntegrityActivationInfo
. . IntegrityProtectionModeInfo
. . . IntegrityProtectionModeCommand
. . . . startIntegrityProtection
. . . . . (BitStringType)integrityProtInitNumber[32] = "00000000000000000000000000000001"
. . . (IntegrityProtectionAlgorithm)integrityProtectionAlgorithm = 0
- Constraint:
ca_CRLC_DL_IntegrityActivateReq
- BinaryMessage:
30 15 02 01 ff 0a 01 01 30 0d 30 30 07 03 05 00 00 00 00 01 0a 01 00

- No.: 1669
- Timestamp: 20:28:55:165_0
- RFN: 3088
- Chip: 20736
- Event: Receive
- PCO: CRLC
- Message: CRLC_Integrity_Activate_CNF
- Source: ts_CRLC_DL_Integrity LINE 2
- Message Structure:
CRLC_Integrity_Activate_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_IntegrityActivateCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1676
- Timestamp: 20:28:55:169_0
- RFN: 3088
- Chip: 37888
- Event: Send
- PCO: CRLC
- Message: CRLC_Integrity_Activate_REQ
- Source: ts_RB2_UL_IntegrityActivate LINE 1
- Message Structure:
CRLC_Integrity_Activate_REQ
. (IntegerType)cellId = -1
. (CN_DomainIdentity)cn_DomainIdentity = 1
. IntegrityActivationInfo
. . IntegrityProtActivationInfoList
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity = 2
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
- Constraint:
ca_CRLC_UL_IntegrityActivateReq
- BinaryMessage:
30 10 02 01 ff 0a 01 01 30 08 30 06 02 01 02 02 01 00

- No.: 1677
- Timestamp: 20:28:55:171_0
- RFN: 3089
- Chip: 5888
- Event: Receive
- PCO: CRLC
- Message: CRLC_Integrity_Activate_CNF
- Source: ts_RB2_UL_IntegrityActivate LINE 2
- Message Structure:
CRLC_Integrity_Activate_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_IntegrityActivateCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1683
- Timestamp: 20:28:55:177_0
- RFN: 3089
- Chip: 29952
- Event: Send
- PCO: AM
- Message: RLC_AM_DATA_REQ
- Source: ts_RRC_Security:lt_SendSecurityModeCommand LINE 7
- Message Structure:
RLC_AM_DATA_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. AmConfirmationRequest
. aM_message
. . DL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00000000000000000000000000000000"
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . DL_DCCH_MessageType
. . . . SecurityModeCommand
. . . . . r3
. . . . . . SecurityModeCommand_r3_IEs
. . . . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . . . SecurityCapability
. . . . . . . . (BitStringType)cipheringAlgorithmCap[16] = '0000000000000011'B
. . . . . . . . (BitStringType)integrityProtectionAlgorithmCap[16] = '0000000000000010'B
. . . . . . . CipheringModeInfo
. . . . . . . IntegrityProtectionModeInfo
. . . . . . . . IntegrityProtectionModeCommand
. . . . . . . . . startIntegrityProtection
. . . . . . . . . . (BitStringType)integrityProtInitNumber[32] = "00000000000000000000000000000001"
. . . . . . . . (IntegrityProtectionAlgorithm)integrityProtectionAlgorithm = 0
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity = 1
. . . . . . . InterRAT_UE_SecurityCapList
. . . . . . laterNonCriticalExtensions
- Constraint:
cas_RRC_SecModeCmd
- BinaryMessage:
30 17 02 01 ff 02 01 02 05 00 80 00 00 00 04 04 00 01 80 01 40 00 00 00 30

- No.: 1689
- Timestamp: 20:28:55:303_0
- RFN: 3102
- Chip: 12032
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_IND
- Source: ts_RRC_Security:lt_StartSecurity_UE LINE 8
- Message Structure:
RLC_AM_DATA_IND
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. IntegrityResult
. . (IntegrityStatus)integrityUsed = 0
. aM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "11101101011010000100111100101101"
. . . . (IntegerType)rrc_MessageSequenceNumber = 1
. . . UL_DCCH_MessageType
. . . . SecurityModeComplete
. . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . IntegrityProtActivationInfo
. . . . . . RRC_MessageSequenceNumberList
. . . . . . . (IntegerType)_elem = 0
. . . . . . . (IntegerType)_elem = 0
. . . . . . . (IntegerType)_elem = 0
. . . . . . . (IntegerType)_elem = 0
. . . . . . . (IntegerType)_elem = 0
. . . . . laterNonCriticalExtensions
. . . . . . (BitStringType)securityModeComplete_r3_add_ext = 0
. . . . . . nonCriticalExtensions
- Constraint:
car_RRC_SecModeCmpl
- BinaryMessage:
30 12 02 01 ff 02 01 02 0a 01 00 f6 b4 27 96 8d 21 00 00 00

- No.: 1690
- Timestamp: 20:28:55:304_0
- RFN: 3102
- Chip: 16128
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_Security:lt_StartSecurity_UE LINE 8
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1692
- Timestamp: 20:28:55:309_0
- RFN: 3102
- Chip: 32256
- Event: Send
- PCO: CRLC
- Message: CRLC_Integrity_Activate_REQ
- Source: ts_CRLC_UL_Integrity LINE 1
- Message Structure:
CRLC_Integrity_Activate_REQ
. (IntegerType)cellId = -1
. (CN_DomainIdentity)cn_DomainIdentity = 1
. IntegrityActivationInfo
. . IntegrityProtActivationInfoList
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity = 0
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity = 1
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity = 3
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity = 4
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
- Constraint:
ca_CRLC_UL_IntegrityActivateReq
- BinaryMessage:
30 28 02 01 ff 0a 01 01 30 20 30 06 02 01 00 02 01 00 30 06 02 01 01 02 01 00 30 06 02 01 03 02 01 00 30 06 02 01 04 02 01 00

- No.: 1693
- Timestamp: 20:28:55:311_0
- RFN: 3103
- Chip: 1536
- Event: Receive
- PCO: CRLC
- Message: CRLC_Integrity_Activate_CNF
- Source: ts_CRLC_UL_Integrity LINE 2
- Message Structure:
CRLC_Integrity_Activate_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_IntegrityActivateCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1705
- Timestamp: 20:28:55:317_0
- RFN: 3103
- Chip: 24832
- Event: Send
- PCO: Dc
- Message: RRC_DataReq
- Source: ts_TC_ActivateRB_TestMode LINE 7
- Message Structure:
RRC_DataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[-1] = -
. (SapId)sapId[1] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. ACTIVATERBTESTMODE
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)tCProtocolDiscriminator[4] = '1111'B
. . (MsgType)msgType[8] = '01000100'B
- Constraint:
ca_PS_DataReq
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 0f 44

- No.: 1706
- Timestamp: 20:28:55:317_1
- RFN: 3103
- Chip: 28160
- Event: Start Timer
- Source: ts_TC_ActivateRB_TestMode LINE 7
- Message Structure:
no details available
- Constraint:
t_Dly (5000 Ms)
- BinaryMessage:

- No.: 1710
- Timestamp: 20:28:55:451_0
- RFN: 3117
- Chip: 4096
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_TC_ActivateRB_TestMode LINE 8
- Message Structure:
RRC_DataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. (START_Value)start[0] = -
. ACTIVATERBTESTMODECOMPLETE
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)tCProtocolDiscriminator[4] = '1111'B
. . (MsgType)msgType[8] = '01000101'B
- Constraint:
car_PS_UplinkDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 0f 45

- No.: 1711
- Timestamp: 20:28:55:452_0
- RFN: 3117
- Chip: 7680
- Event: Cancel Timer
- Source: ts_TC_ActivateRB_TestMode LINE 8
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 1712
- Timestamp: 20:28:55:452_1
- RFN: 3117
- Chip: 8448
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_TC_ActivateRB_TestMode LINE 8
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1729
- Timestamp: 20:28:55:466_0
- RFN: 3118
- Chip: 24064
- Event: Send
- PCO: CPHY
- Message: CPHY_Frame_Number_REQ
- Source: ts_RRC_SetUpRAB_UM_7_RLC LINE 2
- Message Structure:
CPHY_Frame_Number_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
cas_GetFrameNum
- BinaryMessage:
30 06 02 01 00 02 01 1a

- No.: 1733
- Timestamp: 20:28:55:473_0
- RFN: 3119
- Chip: 12032
- Event: Receive
- PCO: CPHY
- Message: CPHY_Frame_Number_CNF
- Source: ts_RRC_SetUpRAB_UM_7_RLC LINE 3
- Message Structure:
CPHY_Frame_Number_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
. (IntegerType)frameNumber = 46
- Constraint:
car_GetFrameNum
- BinaryMessage:
30 09 02 01 00 02 01 1a 02 01 2e

- No.: 1737
- Timestamp: 20:28:55:514_0
- RFN: 3123
- Chip: 16896
- Event: Send
- PCO: AM
- Message: RLC_AM_DATA_REQ
- Source: ts_RRC_SetUpRAB_UM_7_RLC:lt_SendRAB_SetupCS_OrPS LINE 4
- Message Structure:
RLC_AM_DATA_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. AmConfirmationRequest
. . (IntegerType)confirmationRequested = 0
. aM_message
. . DL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00000000000000000000000000000000"
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . DL_DCCH_MessageType
. . . . RadioBearerSetup
. . . . . r3
. . . . . . RadioBearerSetup_r3_IEs
. . . . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . . . IntegrityProtectionModeInfo
. . . . . . . CipheringModeInfo
. . . . . . . (IntegerType)activationTime = 32
. . . . . . . U_RNTI
. . . . . . . (BitStringType)new_C_RNTI[16] = -
. . . . . . . (RRC_StateIndicator)rrc_StateIndicator = 0
. . . . . . . (IntegerType)utran_DRX_CycleLengthCoeff = -
. . . . . . . (BitStringType)ura_Identity[0] = -
. . . . . . . CN_InformationInfo
. . . . . . . SRB_InformationSetupList
. . . . . . . RAB_InformationSetupList
. . . . . . . . RAB_InformationSetup
. . . . . . . . . RAB_Info
. . . . . . . . . . RAB_Identity
. . . . . . . . . . . (BitStringType)gsm_MAP_RAB_Identity[8] = '00000101'B
. . . . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = 1
. . . . . . . . . . (BitStringType)nas_Synchronisation_Indicator[0] = -
. . . . . . . . . . (Re_EstablishmentTimer)re_EstablishmentTimer = 0
. . . . . . . . . RB_InformationSetupList
. . . . . . . . . . RB_InformationSetup
. . . . . . . . . . . (IntegerType)rb_Identity = 20
. . . . . . . . . . . PDCP_Info
. . . . . . . . . . . RLC_InfoChoice
. . . . . . . . . . . . RLC_Info
. . . . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . . . UL_UM_RLC_Mode
. . . . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . RB_MappingInfo
. . . . . . . . . . . . RB_MappingOption
. . . . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . . . (IntegerType)dch = 1
. . . . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 7
. . . . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 7
. . . . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . . . (IntegerType)dch = 6
. . . . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 7
. . . . . . . RB_InformationAffectedList
. . . . . . . DL_CounterSynchronisationInfo
. . . . . . . UL_CommonTransChInfo
. . . . . . . . TFC_Subset
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . TFCS
. . . . . . . . . . . ExplicitTFCS_Configuration
. . . . . . . . . . . . TFCS_ReconfAdd
. . . . . . . . . . . . . ctfcSize
. . . . . . . . . . . . . . ctfc4Bit
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . . . . . . . (IntegerType)ctfc4 = 0
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . . . . . . . (IntegerType)ctfc4 = 1
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . . . . . . . (IntegerType)ctfc4 = 2
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . . . . . . . (IntegerType)ctfc4 = 3
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 11
. . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . UL_DeletedTransChInfoList
. . . . . . . UL_AddReconfTransChInfoList
. . . . . . . . UL_AddReconfTransChInformation
. . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType = 0
. . . . . . . . . (IntegerType)transportChannelIdentity = 1
. . . . . . . . . TransportFormatSet
. . . . . . . . . . DedicatedTransChTFS
. . . . . . . . . . . tti
. . . . . . . . . . . . DedicatedDynamicTF_InfoList
. . . . . . . . . . . . . DedicatedDynamicTF_Info
. . . . . . . . . . . . . . rlc_Size
. . . . . . . . . . . . . . . OctetModeRLC_SizeInfoType1
. . . . . . . . . . . . . . . . sizeType2
. . . . . . . . . . . . . . . . . (IntegerType)part1 = 2
. . . . . . . . . . . . . . . . . (IntegerType)part2 = -
. . . . . . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . LogicalChannelList
. . . . . . . . . . . SemistaticTF_Information
. . . . . . . . . . . . ChannelCodingType
. . . . . . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . . . . . (IntegerType)rateMatchingAttribute = 155
. . . . . . . . . . . . (CRC_Size)crc_Size = 3
. . . . . . . . UL_AddReconfTransChInformation
. . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType = 0
. . . . . . . . . (IntegerType)transportChannelIdentity = 5
. . . . . . . . . TransportFormatSet
. . . . . . . . . . DedicatedTransChTFS
. . . . . . . . . . . tti
. . . . . . . . . . . . DedicatedDynamicTF_InfoList
. . . . . . . . . . . . . DedicatedDynamicTF_Info
. . . . . . . . . . . . . . rlc_Size
. . . . . . . . . . . . . . . BitModeRLC_SizeInfo
. . . . . . . . . . . . . . . . sizeType2
. . . . . . . . . . . . . . . . . (IntegerType)part1 = 2
. . . . . . . . . . . . . . . . . (IntegerType)part2 = -
. . . . . . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . LogicalChannelList
. . . . . . . . . . . SemistaticTF_Information
. . . . . . . . . . . . ChannelCodingType
. . . . . . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . . . . . (IntegerType)rateMatchingAttribute = 170
. . . . . . . . . . . . (CRC_Size)crc_Size = 3
. . . . . . . modeSpecificTransChInfo
. . . . . . . . fdd
. . . . . . . . . (IntegerType)cpch_SetID = -
. . . . . . . . . DRAC_StaticInformationList
. . . . . . . DL_CommonTransChInfo
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . dl_Parameters
. . . . . . . DL_DeletedTransChInfoList
. . . . . . . DL_AddReconfTransChInfoList
. . . . . . . . DL_AddReconfTransChInformation
. . . . . . . . . (DL_TrCH_Type)dl_TransportChannelType = 0
. . . . . . . . . (IntegerType)dl_transportChannelIdentity = 6
. . . . . . . . . tfs_SignallingMode
. . . . . . . . . . UL_TransportChannelIdentity
. . . . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType = 0
. . . . . . . . . . . (IntegerType)ul_TransportChannelIdentity = 1
. . . . . . . . . QualityTarget
. . . . . . . . . . (IntegerType)bler_QualityValue = -20
. . . . . . . . . TM_SignallingInfo
. . . . . . . . DL_AddReconfTransChInformation
. . . . . . . . . (DL_TrCH_Type)dl_TransportChannelType = 0
. . . . . . . . . (IntegerType)dl_transportChannelIdentity = 10
. . . . . . . . . tfs_SignallingMode
. . . . . . . . . . UL_TransportChannelIdentity
. . . . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType = 0
. . . . . . . . . . . (IntegerType)ul_TransportChannelIdentity = 5
. . . . . . . . . QualityTarget
. . . . . . . . . . (IntegerType)bler_QualityValue = -20
. . . . . . . . . TM_SignallingInfo
. . . . . . . FrequencyInfo
. . . . . . . (IntegerType)maxAllowedUL_TX_Power = 33
. . . . . . . UL_ChannelRequirement
. . . . . . . . UL_DPCH_Info
. . . . . . . . . UL_DPCH_PowerControlInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (IntegerType)dpcch_PowerOffset = -40
. . . . . . . . . . . (IntegerType)pc_Preamble = 1
. . . . . . . . . . . (IntegerType)sRB_delay = 7
. . . . . . . . . . . PowerControlAlgorithm
. . . . . . . . . . . . (IntegerType)algorithm1 = 1
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (ScramblingCodeType)scramblingCodeType = 1
. . . . . . . . . . . (IntegerType)scramblingCode = 0
. . . . . . . . . . . (IntegerType)numberOfDPDCH = -
. . . . . . . . . . . (SpreadingFactor)spreadingFactor = 4
. . . . . . . . . . . (BooleanType)tfci_Existence = TRUE
. . . . . . . . . . . (IntegerType)numberOfFBI_Bits = -
. . . . . . . . . . . (PuncturingLimit)puncturingLimit = 15
. . . . . . . modeSpecificPhysChInfo
. . . . . . . . fdd
. . . . . . . . . DL_PDSCH_Information
. . . . . . . DL_CommonInformation
. . . . . . . . DL_DPCH_InfoCommon
. . . . . . . . . cfnHandling
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . DL_DPCH_PowerControlInfo
. . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . (DPC_Mode)dpc_Mode = 0
. . . . . . . . . . . (IntegerType)powerOffsetPilot_pdpdch = 0
. . . . . . . . . . . Dl_rate_matching_restriction
. . . . . . . . . . . SF512_AndPilot
. . . . . . . . . . . . (PilotBits128)sfd128 = 0
. . . . . . . . . . . (PositionFixedOrFlexible)positionFixedOrFlexible = 1
. . . . . . . . . . . (BooleanType)tfci_Existence = TRUE
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . (IntegerType)defaultDPCH_OffsetValue = -
. . . . . . . . . . DPCH_CompressedModeInfo
. . . . . . . . . . (TX_DiversityMode)tx_DiversityMode = 0
. . . . . . . . . . SSDT_Information
. . . . . . . DL_InformationPerRL_List
. . . . . . . . DL_InformationPerRL
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . PrimaryCPICH_Info
. . . . . . . . . . . . (IntegerType)primaryScramblingCode = 100
. . . . . . . . . . . PDSCH_SHO_DCH_Info
. . . . . . . . . . . PDSCH_CodeMapping
. . . . . . . . . DL_DPCH_InfoPerRL
. . . . . . . . . . fdd
. . . . . . . . . . . (PCPICH_UsageForChannelEst)pCPICH_UsageForChannelEst = 0
. . . . . . . . . . . (IntegerType)dpch_FrameOffset = 0
. . . . . . . . . . . SecondaryCPICH_Info
. . . . . . . . . . . DL_ChannelisationCodeList
. . . . . . . . . . . . DL_ChannelisationCode
. . . . . . . . . . . . . (IntegerType)secondaryScramblingCode = 1
. . . . . . . . . . . . . SF512_AndCodeNumber
. . . . . . . . . . . . . . (IntegerType)sf128 = 0
. . . . . . . . . . . . . (ScramblingCodeChange)scramblingCodeChange = -
. . . . . . . . . . . (IntegerType)tpc_CombinationIndex = 0
. . . . . . . . . . . (SSDT_CellIdentity)ssdt_CellIdentity = -
. . . . . . . . . . . (ClosedLoopTimingAdjMode)closedLoopTimingAdjMode = -
. . . . . . . . . SCCPCH_InfoForFACH
. . . . . . v3a0NonCriticalExtensions
. . . . . . . RadioBearerSetup_v3a0ext
. . . . . . . . (BitStringType)new_DSCH_RNTI[16] = -
. . . . . . . laterNonCriticalExtensions
- Constraint:
cas_RB_SetUpAM_WithCnf
- BinaryMessage:
30 4a 02 01 ff 02 01 02 02 01 00 80 00 00 00 03 92 04 ba f0 80 00 16 09 b4 8d 00 ce 42 b1 02 01 c1 22 92 49 95 f8 10 08 14 20 88 e6 98 84 02 20 88 ea 58 30 c2 c0 ae 26 25 74 d2 a3 d1 00 00 00 9f 24 02 b1 02 06 40 00 08 28 00 00

- No.: 1742
- Timestamp: 20:28:55:701_0
- RFN: 3142
- Chip: 2560
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_CNF
- Source: ts_RRC_SetUpRAB_UM_7_RLC LINE 6
- Message Structure:
RLC_AM_DATA_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. (IntegerType)mui = 0
- Constraint:
car_AM_DataMuiCnf
- BinaryMessage:
30 09 02 01 ff 02 01 02 02 01 00

- No.: 1749
- Timestamp: 20:28:55:833_0
- RFN: 3155
- Chip: 12288
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Modify_REQ
- Source: ts_SS_2DCH_Modify LINE 3
- Message Structure:
CPHY_RL_Modify_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
. (RatType)ratType = 0
. CphyRlModifyReq
. . SS_ActivationTime
. . . (IntegerType)activationCFN = 32
. . physicalChannelInfo
. . . DPCHInfo
. . . . UL_DPCH_Info
. . . . DL_DPCHInfo
. . . . . DL_CommonInformation
. . . . . . DL_DPCH_InfoCommon
. . . . . . . cfnHandling
. . . . . . . modeSpecificInfo
. . . . . . . . fdd
. . . . . . . . . DL_DPCH_PowerControlInfo
. . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . fdd
. . . . . . . . . . . . (DPC_Mode)dpc_Mode = 0
. . . . . . . . . (IntegerType)powerOffsetPilot_pdpdch = 0
. . . . . . . . . Dl_rate_matching_restriction
. . . . . . . . . SF512_AndPilot
. . . . . . . . . . (PilotBits128)sfd128 = 0
. . . . . . . . . (PositionFixedOrFlexible)positionFixedOrFlexible = 1
. . . . . . . . . (BooleanType)tfci_Existence = TRUE
. . . . . . modeSpecificInfo
. . . . . . . fdd
. . . . . . . . (IntegerType)defaultDPCH_OffsetValue = -
. . . . . . . . DPCH_CompressedModeInfo
. . . . . . . . (TX_DiversityMode)tx_DiversityMode = 0
. . . . . . . . SSDT_Information
. . . . . DL_DPCH_InfoPerRL
. . . . . . fdd
. . . . . . . (PCPICH_UsageForChannelEst)pCPICH_UsageForChannelEst = 0
. . . . . . . (IntegerType)dpch_FrameOffset = 0
. . . . . . . SecondaryCPICH_Info
. . . . . . . DL_ChannelisationCodeList
. . . . . . . . DL_ChannelisationCode
. . . . . . . . . (IntegerType)secondaryScramblingCode = 1
. . . . . . . . . SF512_AndCodeNumber
. . . . . . . . . . (IntegerType)sf128 = 0
. . . . . . . . . (ScramblingCodeChange)scramblingCodeChange = -
. . . . . . . (IntegerType)tpc_CombinationIndex = 0
. . . . . . . (SSDT_CellIdentity)ssdt_CellIdentity = -
. . . . . . . (ClosedLoopTimingAdjMode)closedLoopTimingAdjMode = -
. . . . . (IntegerType)powerOffsetOfTFCI_PO1 = 0
. . . . . (IntegerType)powerOffsetOfTPC_PO2 = 0
. . . . . (IntegerType)powerOffsetOfPILOT_PO3 = 0
. . . . . (IntegerType)dl_TxPower = -5
. . . . . (IntegerType)dl_TxPowerMax = 15
. . . . . (IntegerType)dl_TxPowerMin = -35
- Constraint:
ca_DL_DPCH_ModifyInfo
- BinaryMessage:
30 5d 02 01 00 02 01 1a 0a 01 00 30 52 02 01 20 30 4d 30 4b 30 21 30 19 05 00 30 30 14 30 06 30 30 03 0a 01 00 02 01 00 0a 01 00 0a 01 01 01 01 ff 30 30 03 0a 01 00 30 30 13 0a 01 00 02 01 00 30 08 30 06 02 01 01 02 01 00 02 01 00 02 01 00 02 01 00 02 01 00 02 01 fb 02 01 0f 02 01 dd

- No.: 1753
- Timestamp: 20:28:55:882_0
- RFN: 3160
- Chip: 5120
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Modify_CNF
- Source: ts_SS_2DCH_Modify LINE 4
- Message Structure:
CPHY_RL_Modify_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
ca_RL_ModifyCnf
- BinaryMessage:
30 06 02 01 00 02 01 1a

- No.: 1754
- Timestamp: 20:28:55:908_0
- RFN: 3162
- Chip: 30464
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Config_REQ
- Source: ts_SS_2DCH_Modify LINE 5
- Message Structure:
CPHY_TrCH_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
. (RatType)ratType = 0
. CphyTrchConfigReq
. . SS_ActivationTime
. . . (IntegerType)activationCFN = 32
. . ulconnectedTrCHList
. . TFCS
. . dlconnectedTrCHList
. . . CphyTrchConfigReq_setseq_1
. . . . (IntegerType)trchid = 6
. . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 336
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional = 1
. . . . . . (IntegerType)rateMatchingAttribute = 155
. . . . . . (CRC_Size)crc_Size = 3
. . . CphyTrchConfigReq_setseq_1
. . . . (IntegerType)trchid = 10
. . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 148
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional = 1
. . . . . . (IntegerType)rateMatchingAttribute = 170
. . . . . . (CRC_Size)crc_Size = 3
. . TFCS
. . . ExplicitTFCS_Configuration
. . . . TFCS_ReconfAdd
. . . . . ctfcSize
. . . . . . ctfc4Bit
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 0
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 1
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 2
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 3
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . fdd
. . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 9
. . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
- Constraint:
ca_TrChCfgInfo
- BinaryMessage:
30 81 95 02 01 00 02 01 1a 0a 01 00 30 81 89 02 01 20 30 4c 30 24 02 01 06 0a 01 00 30 1c 30 0e 30 0c 02 02 01 50 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 9b 0a 01 03 30 24 02 01 0a 0a 01 00 30 1c 30 0e 30 0c 02 02 00 94 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 aa 0a 01 03 30 36 30 30 33 30 08 02 01 00 30 03 02 01 00 30 08 02 01 01 30 03 02 01 00 30 08 02 01 02 30 03 02 01 00 30 13 02 01 03 30 0e 30 0c 30 30 03 02 01 09 02 01 0f 02 01 00

- No.: 1758
- Timestamp: 20:28:55:961_0
- RFN: 3168
- Chip: 3328
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Config_CNF
- Source: ts_SS_2DCH_Modify LINE 6
- Message Structure:
CPHY_TrCH_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
ca_TrChCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 1a

- No.: 1759
- Timestamp: 20:28:56:023_0
- RFN: 3174
- Chip: 11776
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_SS_2DCH_Modify LINE 7
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
. (RatType)ratType = 0
. configMessage
. . CmacConfigReq
. . . SS_ActivationTime
. . . . (IntegerType)activationCFN = 32
. . . UE_Info
. . . . U_RNTI
. . . . (BitStringType)c_RNTI[16] = -
. . . TrCHInfo
. . . . ulconnectedTrCHList
. . . . TFCS
. . . . dlconnectedTrCHList
. . . . . TrCHInfo_setseq_1
. . . . . . (IntegerType)trchid = 6
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 336
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . (IntegerType)rateMatchingAttribute = 155
. . . . . . . . (CRC_Size)crc_Size = 3
. . . . . TrCHInfo_setseq_1
. . . . . . (IntegerType)trchid = 10
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 148
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . (IntegerType)rateMatchingAttribute = 170
. . . . . . . . (CRC_Size)crc_Size = 3
. . . . TFCS
. . . . . ExplicitTFCS_Configuration
. . . . . . TFCS_ReconfAdd
. . . . . . . ctfcSize
. . . . . . . . ctfc4Bit
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 0
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 1
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 2
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 3
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 9
. . . . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . TrCH_LogCHMappingList1
. . . . ulconnectedTrCHList
. . . . dlconnectedTrCHList
. . . . . TrCH_LogCHMappingList1_setseq_1
. . . . . . (IntegerType)trchid = 6
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 7
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 5
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 7
. . . . . . . . (IntegerType)rB_Identity = -10
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . TrCH_LogCHMappingList1_setseq_1
. . . . . . (IntegerType)trchid = 10
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 1
. . . . . . . . (IntegerType)rB_Identity = 1
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 2
. . . . . . . . (IntegerType)rB_Identity = 2
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 3
. . . . . . . . (IntegerType)rB_Identity = 3
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 4
. . . . . . . . (IntegerType)rB_Identity = 4
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_CMAC_ReconfigInfo
- BinaryMessage:
30 82 01 21 02 01 ff 02 01 1a 0a 01 00 30 82 01 14 02 01 20 30 00 30 81 80 30 46 30 21 02 01 06 30 1c 30 0e 30 0c 02 02 01 50 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 9b 0a 01 03 30 21 02 01 0a 30 1c 30 0e 30 0c 02 02 00 94 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 aa 0a 01 03 30 36 30 30 33 30 08 02 01 00 30 03 02 01 00 30 08 02 01 01 30 03 02 01 00 30 08 02 01 02 30 03 02 01 00 30 13 02 01 03 30 0e 30 0c 30 30 03 02 01 09 02 01 0f 02 01 00 30 81 89 30 81 86 30 1d 02 01 06 30 18 30 16 30 11 0a 01 00 0a 01 00 02 01 07 0a 01 05 05 00 02 01 07 02 01 f6 30 65 02 01 0a 30 60 30 16 30 11 0a 01 00 0a 01 00 02 01 01 0a 01 04 05 00 02 01 01 02 01 01 30 16 30 11 0a 01 00 0a 01 00 02 01 02 0a 01 04 05 00 02 01 02 02 01 02 30 16 30 11 0a 01 00 0a 01 00 02 01 03 0a 01 04 05 00 02 01 03 02 01 03 30 16 30 11 0a 01 00 0a 01 00 02 01 04 0a 01 04 05 00 02 01 04 02 01 04

- No.: 1760
- Timestamp: 20:28:56:058_0
- RFN: 3177
- Chip: 32768
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_SS_2DCH_Modify LINE 8
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 1a

- No.: 1761
- Timestamp: 20:28:56:086_0
- RFN: 3180
- Chip: 24832
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Modify_REQ
- Source: ts_SS_2DCH_Modify LINE 9
- Message Structure:
CPHY_RL_Modify_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
. (RatType)ratType = 0
. CphyRlModifyReq
. . SS_ActivationTime
. . . (IntegerType)activationCFN = 32
. . physicalChannelInfo
. . . DPCHInfo
. . . . UL_DPCH_Info
. . . . . UL_DPCH_PowerControlInfo
. . . . . . fdd
. . . . . . . (IntegerType)dpcch_PowerOffset = -40
. . . . . . . (IntegerType)pc_Preamble = 1
. . . . . . . (IntegerType)sRB_delay = 7
. . . . . . . PowerControlAlgorithm
. . . . . . . . (IntegerType)algorithm1 = 1
. . . . . modeSpecificInfo
. . . . . . fdd
. . . . . . . (ScramblingCodeType)scramblingCodeType = 1
. . . . . . . (IntegerType)scramblingCode = 0
. . . . . . . (IntegerType)numberOfDPDCH = -
. . . . . . . (SpreadingFactor)spreadingFactor = 4
. . . . . . . (BooleanType)tfci_Existence = TRUE
. . . . . . . (IntegerType)numberOfFBI_Bits = -
. . . . . . . (PuncturingLimit)puncturingLimit = 15
. . . . DL_DPCHInfo
- Constraint:
ca_UL_DPCH_ModifyInfo
- BinaryMessage:
30 33 02 01 00 02 01 14 0a 01 00 30 28 02 01 20 30 23 30 21 30 30 0c 02 01 d8 02 01 01 02 01 07 02 01 01 30 30 0f 0a 01 01 02 01 00 0a 01 04 01 01 ff 0a 01 0f

- No.: 1765
- Timestamp: 20:28:56:137_0
- RFN: 3185
- Chip: 29696
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Modify_CNF
- Source: ts_SS_2DCH_Modify LINE 10
- Message Structure:
CPHY_RL_Modify_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_RL_ModifyCnf
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 1766
- Timestamp: 20:28:56:167_0
- RFN: 3188
- Chip: 29184
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Config_REQ
- Source: ts_SS_2DCH_Modify LINE 11
- Message Structure:
CPHY_TrCH_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
. (RatType)ratType = 0
. CphyTrchConfigReq
. . SS_ActivationTime
. . . (IntegerType)activationCFN = 32
. . ulconnectedTrCHList
. . . CphyTrchConfigReq_setseq_0
. . . . (IntegerType)trchid = 1
. . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 336
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional = 1
. . . . . . (IntegerType)rateMatchingAttribute = 155
. . . . . . (CRC_Size)crc_Size = 3
. . . CphyTrchConfigReq_setseq_0
. . . . (IntegerType)trchid = 5
. . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 148
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional = 1
. . . . . . (IntegerType)rateMatchingAttribute = 170
. . . . . . (CRC_Size)crc_Size = 3
. . TFCS
. . . ExplicitTFCS_Configuration
. . . . TFCS_ReconfAdd
. . . . . ctfcSize
. . . . . . ctfc4Bit
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 0
. . . . . . . . PowerOffsetInformation
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 1
. . . . . . . . PowerOffsetInformation
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 2
. . . . . . . . PowerOffsetInformation
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 3
. . . . . . . . PowerOffsetInformation
. . dlconnectedTrCHList
. . TFCS
- Constraint:
ca_TrChCfgInfo
- BinaryMessage:
30 75 02 01 00 02 01 14 0a 01 00 30 6a 02 01 20 30 4c 30 24 02 01 01 0a 01 00 30 1c 30 0e 30 0c 02 02 01 50 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 9b 0a 01 03 30 24 02 01 05 0a 01 00 30 1c 30 0e 30 0c 02 02 00 94 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 aa 0a 01 03 30 17 30 30 14 30 03 02 01 00 30 03 02 01 01 30 03 02 01 02 30 03 02 01 03

- No.: 1770
- Timestamp: 20:28:56:220_0
- RFN: 3194
- Chip: 0
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Config_CNF
- Source: ts_SS_2DCH_Modify LINE 12
- Message Structure:
CPHY_TrCH_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_TrChCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 1771
- Timestamp: 20:28:56:285_0
- RFN: 3200
- Chip: 17664
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_SS_2DCH_Modify LINE 13
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
. (RatType)ratType = 0
. configMessage
. . CmacConfigReq
. . . SS_ActivationTime
. . . . (IntegerType)activationCFN = 32
. . . UE_Info
. . . . U_RNTI
. . . . (BitStringType)c_RNTI[16] = -
. . . TrCHInfo
. . . . ulconnectedTrCHList
. . . . . TrCHInfo_setseq_0
. . . . . . (IntegerType)trchid = 1
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 336
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . (IntegerType)rateMatchingAttribute = 155
. . . . . . . . (CRC_Size)crc_Size = 3
. . . . . TrCHInfo_setseq_0
. . . . . . (IntegerType)trchid = 5
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 148
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . (IntegerType)rateMatchingAttribute = 170
. . . . . . . . (CRC_Size)crc_Size = 3
. . . . TFCS
. . . . . ExplicitTFCS_Configuration
. . . . . . TFCS_ReconfAdd
. . . . . . . ctfcSize
. . . . . . . . ctfc4Bit
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 0
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 1
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 2
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 3
. . . . . . . . . . PowerOffsetInformation
. . . . dlconnectedTrCHList
. . . . TFCS
. . . TrCH_LogCHMappingList1
. . . . ulconnectedTrCHList
. . . . . TrCH_LogCHMappingList1_setseq_0
. . . . . . (IntegerType)trchid = 1
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 7
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 5
. . . . . . . . (IntegerType)rB_Identity = -10
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . TrCH_LogCHMappingList1_setseq_0
. . . . . . (IntegerType)trchid = 5
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . (IntegerType)rB_Identity = 1
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . (IntegerType)rB_Identity = 2
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . (IntegerType)rB_Identity = 3
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . (IntegerType)rB_Identity = 4
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . dlconnectedTrCHList
- Constraint:
ca_CMAC_ReconfigInfo
- BinaryMessage:
30 81 e5 02 01 ff 02 01 14 0a 01 00 30 81 d9 02 01 20 30 00 30 61 30 46 30 21 02 01 01 30 1c 30 0e 30 0c 02 02 01 50 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 9b 0a 01 03 30 21 02 01 05 30 1c 30 0e 30 0c 02 02 00 94 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 aa 0a 01 03 30 17 30 30 14 30 03 02 01 00 30 03 02 01 01 30 03 02 01 02 30 03 02 01 03 30 6f 30 6d 30 18 02 01 01 30 13 30 11 30 0c 0a 01 00 0a 01 00 02 01 07 0a 01 05 02 01 f6 30 51 02 01 05 30 4c 30 11 30 0c 0a 01 00 0a 01 00 02 01 01 0a 01 04 02 01 01 30 11 30 0c 0a 01 00 0a 01 00 02 01 02 0a 01 04 02 01 02 30 11 30 0c 0a 01 00 0a 01 00 02 01 03 0a 01 04 02 01 03 30 11 30 0c 0a 01 00 0a 01 00 02 01 04 0a 01 04 02 01 04

- No.: 1772
- Timestamp: 20:28:56:318_0
- RFN: 3203
- Chip: 30976
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_SS_2DCH_Modify LINE 14
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 14

- No.: 1775
- Timestamp: 20:28:56:328_0
- RFN: 3204
- Chip: 29440
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB_TM_Cfg_RLC LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = -10
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_TM_RLC_Mode
. . . . . . (BooleanType)segmentationIndication = TRUE
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 336
. . . . . UL_RLC_Mode
. . . . . . UL_TM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . (BooleanType)segmentationIndication = TRUE
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = 7
. . . . (IntegerType)dLlogicalChannelIdentity = 7
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_TM_Info
- BinaryMessage:
30 25 02 01 ff 02 01 f6 0a 01 00 30 1a 30 10 30 03 01 01 ff 30 09 02 02 01 50 30 03 01 01 ff 30 06 02 01 07 02 01 07

- No.: 1779
- Timestamp: 20:28:56:340_0
- RFN: 3206
- Chip: 0
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB_TM_Cfg_RLC LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = -10
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 f6

- No.: 1787
- Timestamp: 20:28:56:345_1
- RFN: 3206
- Chip: 20224
- Event: Start Timer
- Source: ts_RRC_ReceiveRB_SetupCmpl LINE 2
- Message Structure:
no details available
- Constraint:
t_WaitMS (13500 Ms)
- BinaryMessage:

- No.: 1796
- Timestamp: 20:28:57:987_0
- RFN: 3370
- Chip: 28928
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_IND
- Source: ts_RRC_ReceiveRB_SetupCmpl:lt_CipheringNotStartedAM_RAB LINE 4
- Message Structure:
RLC_AM_DATA_IND
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. IntegrityResult
. . (IntegrityStatus)integrityUsed = 0
. aM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "01100111110100110110111001101110"
. . . . (IntegerType)rrc_MessageSequenceNumber = 2
. . . UL_DCCH_MessageType
. . . . RadioBearerSetupComplete
. . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . IntegrityProtActivationInfo
. . . . . (IntegerType)ul_TimingAdvance = 0
. . . . . (BitStringType)start_Value[20] = "00000000000000000100"
. . . . . (IntegerType)count_C_ActivationTime = 0
. . . . . UL_CounterSynchronisationInfo
. . . . . laterNonCriticalExtensions
. . . . . . (BitStringType)radioBearerSetupComplete_r3_add_ext = 0
. . . . . . nonCriticalExtensions
- Constraint:
car_RB_SetUpCmpl
- BinaryMessage:
30 12 02 01 ff 02 01 02 0a 01 00 b3 e9 b7 37 13 c8 00 00 08

- No.: 1797
- Timestamp: 20:28:57:989_0
- RFN: 3370
- Chip: 34560
- Event: Cancel Timer
- Source: ts_RRC_ReceiveRB_SetupCmpl:lt_CipheringNotStartedAM_RAB LINE 4
- Message Structure:
no details available
- Constraint:
t_WaitMS
- BinaryMessage:

- No.: 1798
- Timestamp: 20:28:57:989_1
- RFN: 3370
- Chip: 35328
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ReceiveRB_SetupCmpl:lt_CipheringNotStartedAM_RAB LINE 4
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1822
- Timestamp: 20:28:58:007_0
- RFN: 3372
- Chip: 28672
- Event: Send
- PCO: Dc
- Message: RRC_DataReq
- Source: ts_TC_CloseUE_TestLoop LINE 6
- Message Structure:
RRC_DataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[-1] = -
. (SapId)sapId[1] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. CLOSEUETESTLOOP
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)tCProtocolDiscriminator[4] = '1111'B
. . (MsgType)msgType[8] = '01000000'B
. . (UE_TestLoopMode)uE_TestLoopMode[1] = '00'O
. . UE_TestLoopMode1LB_Setup
. . . (Length)iel[1] = '03'O
. . . LB_SetupRB_IE
. . . . (BitStringType)rLC_SDU_Size[16] = '0000000101010000'B
. . . . (BitStringType)spare_2[3] = '000'B
. . . . (BitStringType)rB_Identity[5] = '10100'B
. . . LB_SetupRB_IE
. . . LB_SetupRB_IE
. . . LB_SetupRB_IE
- Constraint:
ca_PS_DataReq
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 0f 40 00 03 01 50 14

- No.: 1823
- Timestamp: 20:28:58:008_0
- RFN: 3372
- Chip: 34048
- Event: Start Timer
- Source: ts_TC_CloseUE_TestLoop LINE 6
- Message Structure:
no details available
- Constraint:
t_Dly (5000 Ms)
- BinaryMessage:

- No.: 1827
- Timestamp: 20:28:58:301_0
- RFN: 3402
- Chip: 3840
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_TC_CloseUE_TestLoop LINE 7
- Message Structure:
RRC_DataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. (START_Value)start[0] = -
. CLOSEUETESTLOOPCOMPLETE
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)tCProtocolDiscriminator[4] = '1111'B
. . (MsgType)msgType[8] = '01000001'B
- Constraint:
car_PS_UplinkDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 0f 41

- No.: 1828
- Timestamp: 20:28:58:301_1
- RFN: 3402
- Chip: 7168
- Event: Cancel Timer
- Source: ts_TC_CloseUE_TestLoop LINE 7
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 1829
- Timestamp: 20:28:58:302_0
- RFN: 3402
- Chip: 7936
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_TC_CloseUE_TestLoop LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1851
- Timestamp: 20:28:58:318_0
- RFN: 3403
- Chip: 32000
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxUMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -10
. UMD_PDU
. . UMD_PDU_MSG
. . . (UM_SeqNum)seqNum[7] = '0000000'B
. . . (ExtBit)eBit[1] = '0'B
. . . LenInds
. . . (UM_Data)data[-1] = 'FFE665A5C5CA3452085408ABEECE4B0B813FD337873F2CD1E29AE91BD6C8E14FDE630F8195688EBE46'O
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f6 00 ff e6 65 a5 c5 ca 34 52 08 54 08 ab ee ce 4b 0b 81 3f d3 37 87 3f 2c d1 e2 9a e9 1b d6 c8 e1 4f de 63 0f 81 95 68 8e be 46

- No.: 1876
- Timestamp: 20:28:58:330_0
- RFN: 3405
- Chip: 2816
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxUMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -10
. UMD_PDU
. . UMD_PDU_MSG
. . . (UM_SeqNum)seqNum[7] = '0000001'B
. . . (ExtBit)eBit[1] = '1'B
. . . LenInds
. . . . LenInd7AndE_Bit
. . . . . (LenInd7)lenInd[7] = '0000001'B
. . . . . (ExtBit)extBit[1] = '0'B
. . . . LenInd7AndE_Bit
. . . . LenInd7AndE_Bit
. . . . LenInd7AndE_Bit
. . . . LenInd7AndE_Bit
. . . . LenInd15AndE_Bit
. . . . LenInd15AndE_Bit
. . . . LenInd15AndE_Bit
. . . (UM_Data)data[-1] = '5F09816A8EEB1B83953DD362DAE3B06D5B76D8E3E53087EA645A09017FD99C3CACBB46DF1CD61DA9'O
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f6 03 02 5f 09 81 6a 8e eb 1b 83 95 3d d3 62 da e3 b0 6d 5b 76 d8 e3 e5 30 87 ea 64 5a 09 01 7f d9 9c 3c ac bb 46 df 1c d6 1d a9

- No.: 1901
- Timestamp: 20:28:58:342_0
- RFN: 3406
- Chip: 10496
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxUMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -10
. UMD_PDU
. . UMD_PDU_MSG
. . . (UM_SeqNum)seqNum[7] = '0000010'B
. . . (ExtBit)eBit[1] = '1'B
. . . LenInds
. . . . LenInd7AndE_Bit
. . . . . (LenInd7)lenInd[7] = '0101001'B
. . . . . (ExtBit)extBit[1] = '0'B
. . . . LenInd7AndE_Bit
. . . . LenInd7AndE_Bit
. . . . LenInd7AndE_Bit
. . . . LenInd7AndE_Bit
. . . . LenInd15AndE_Bit
. . . . LenInd15AndE_Bit
. . . . LenInd15AndE_Bit
. . . (UM_Data)data[-1] = 'C435F89943DF9CC34ADEE31AD6E24FA1903D53778D949742750DD49DE9CE9E430AD448A14575D89C'O
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f6 05 52 c4 35 f8 99 43 df 9c c3 4a de e3 1a d6 e2 4f a1 90 3d 53 77 8d 94 97 42 75 0d d4 9d e9 ce 9e 43 0a d4 48 a1 45 75 d8 9c

- No.: 1927
- Timestamp: 20:28:58:355_0
- RFN: 3407
- Chip: 19712
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxUMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -10
. UMD_PDU
. . UMD_PDU_MSG
. . . (UM_SeqNum)seqNum[7] = '0000011'B
. . . (ExtBit)eBit[1] = '1'B
. . . LenInds
. . . . LenInd7AndE_Bit
. . . . . (LenInd7)lenInd[7] = '0000101'B
. . . . . (ExtBit)extBit[1] = '1'B
. . . . LenInd7AndE_Bit
. . . . . (LenInd7)lenInd[7] = '1111111'B
. . . . . (ExtBit)extBit[1] = '0'B
. . . . LenInd7AndE_Bit
. . . . LenInd7AndE_Bit
. . . . LenInd7AndE_Bit
. . . . LenInd15AndE_Bit
. . . . LenInd15AndE_Bit
. . . . LenInd15AndE_Bit
. . . (UM_Data)data[-1] = '1602550881'O
. . (Padding)padding[-1] = '00000000000000000000000000000000000000000000000000000000000000000000'H
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f6 07 0b fe 16 02 55 08 81 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00

- No.: 1958
- Timestamp: 20:28:58:581_0
- RFN: 3430
- Chip: 5376
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: ts_RxUMD_PRBS LINE 5
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -10
. UMD_PDU
. . UMD_PDU_MSG
. . . (UM_SeqNum)seqNum[7] = '0000000'B
. . . (ExtBit)eBit[1] = '0'B
. . . LenInds
. . . (UM_Data)data[41] = 'FFE665A5C5CA3452085408ABEECE4B0B813FD337873F2CD1E29AE91BD6C8E14FDE630F8195688EBE46'O
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f6 00 ff e6 65 a5 c5 ca 34 52 08 54 08 ab ee ce 4b 0b 81 3f d3 37 87 3f 2c d1 e2 9a e9 1b d6 c8 e1 4f de 63 0f 81 95 68 8e be 46

- No.: 1987
- Timestamp: 20:28:58:624_0
- RFN: 3434
- Chip: 17408
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: ts_RxUMD_PRBS LINE 6
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -10
. UMD_PDU
. . UMD_PDU_MSG
. . . (UM_SeqNum)seqNum[7] = '0000001'B
. . . (ExtBit)eBit[1] = '1'B
. . . LenInds
. . . . LenInd7AndE_Bit
. . . . . (LenInd7)lenInd[7] = '0000001'B
. . . . . (ExtBit)extBit[1] = '1'B
. . . . LenInd7AndE_Bit
. . . . . (LenInd7)lenInd[7] = '1111111'B
. . . . . (ExtBit)extBit[1] = '0'B
. . . . LenInd7AndE_Bit
. . . . LenInd7AndE_Bit
. . . . LenInd7AndE_Bit
. . . . LenInd15AndE_Bit
. . . . LenInd15AndE_Bit
. . . . LenInd15AndE_Bit
. . . (UM_Data)data[1] = '5F'O
. . (Padding)padding[76] = '5555555555555555555555555555555555555555555555555555555555555555555555555555'H
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f6 03 03 fe 5f 55 55 55 55 55 55 55 55 55 55 55 55 55 55 55 55 55 55 55 55 55 55 55 55 55 55 55 55 55 55 55 55 55 55 55 55 55 55

- No.: 1991
- Timestamp: 20:28:58:627_0
- RFN: 3434
- Chip: 26624
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: tc_7_2_2_6 LINE 12
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1998
- Timestamp: 20:28:58:631_0
- RFN: 3435
- Chip: 4352
- Event: Send
- PCO: Dc
- Message: RRC_DataReq
- Source: ts_TC_OpenUE_TestLoop LINE 6
- Message Structure:
RRC_DataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[-1] = -
. (SapId)sapId[1] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. OPENUETESTLOOP
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)tCProtocolDiscriminator[4] = '1111'B
. . (MsgType)msgType[8] = '01000010'B
- Constraint:
ca_PS_DataReq
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 0f 42

- No.: 1999
- Timestamp: 20:28:58:632_0
- RFN: 3435
- Chip: 7936
- Event: Start Timer
- Source: ts_TC_OpenUE_TestLoop LINE 6
- Message Structure:
no details available
- Constraint:
t_Dly (5000 Ms)
- BinaryMessage:

- No.: 2003
- Timestamp: 20:28:58:901_0
- RFN: 3462
- Chip: 4608
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_TC_OpenUE_TestLoop LINE 7
- Message Structure:
RRC_DataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. (START_Value)start[0] = -
. OPENUETESTLOOPCOMPLETE
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)tCProtocolDiscriminator[4] = '1111'B
. . (MsgType)msgType[8] = '01000011'B
- Constraint:
car_PS_UplinkDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 0f 43

- No.: 2004
- Timestamp: 20:28:58:902_0
- RFN: 3462
- Chip: 7936
- Event: Cancel Timer
- Source: ts_TC_OpenUE_TestLoop LINE 7
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 2005
- Timestamp: 20:28:58:902_1
- RFN: 3462
- Chip: 8704
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_TC_OpenUE_TestLoop LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2013
- Timestamp: 20:28:58:907_0
- RFN: 3462
- Chip: 28672
- Event: Send
- PCO: Dc
- Message: RRC_DataReq
- Source: ts_TC_DeactivateRB_TestMode LINE 6
- Message Structure:
RRC_DataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[-1] = -
. (SapId)sapId[1] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. DEACTIVATERBTESTMODE
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)tCProtocolDiscriminator[4] = '1111'B
. . (MsgType)msgType[8] = '01000110'B
- Constraint:
ca_PS_DataReq
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 0f 46

- No.: 2014
- Timestamp: 20:28:58:908_0
- RFN: 3462
- Chip: 32000
- Event: Start Timer
- Source: ts_TC_DeactivateRB_TestMode LINE 6
- Message Structure:
no details available
- Constraint:
t_Dly (5000 Ms)
- BinaryMessage:

- No.: 2018
- Timestamp: 20:28:59:221_0
- RFN: 3494
- Chip: 4608
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_TC_DeactivateRB_TestMode LINE 7
- Message Structure:
RRC_DataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. (START_Value)start[0] = -
. DEACTIVATERBTESTMODECOMPLETE
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)tCProtocolDiscriminator[4] = '1111'B
. . (MsgType)msgType[8] = '01000111'B
- Constraint:
car_PS_UplinkDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 0f 47

- No.: 2019
- Timestamp: 20:28:59:222_0
- RFN: 3494
- Chip: 7680
- Event: Cancel Timer
- Source: ts_TC_DeactivateRB_TestMode LINE 7
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 2020
- Timestamp: 20:28:59:222_1
- RFN: 3494
- Chip: 8448
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_TC_DeactivateRB_TestMode LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2032
- Timestamp: 20:28:59:230_0
- RFN: 3494
- Chip: 37888
- Event: Send
- PCO: UM
- Message: RLC_UM_DATA_REQ
- Source: po_ConnectionAndSS_Rel:lt_Send_RRC_ConnectionRelease LINE 8
- Message Structure:
RLC_UM_DATA_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. uM_message
. . DL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00000000000000000000000000000000"
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . DL_DCCH_MessageType
. . . . RRCConnectionRelease
. . . . . r3
. . . . . . RRCConnectionRelease_r3_IEs
. . . . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . . . (IntegerType)n_308 = 1
. . . . . . . (ReleaseCause)releaseCause = 0
. . . . . . . Rplmn_Information
. . . . . . laterNonCriticalExtensions
. (BooleanType)specialLI = FALSE
- Constraint:
cas_RRC_ConnRelDCCH
- BinaryMessage:
30 10 02 01 ff 02 01 01 80 00 00 00 03 c8 00 01 01 00

- No.: 2036
- Timestamp: 20:28:59:462_0
- RFN: 3518
- Chip: 8192
- Event: Receive
- PCO: UM
- Message: RLC_UM_DATA_IND
- Source: po_ConnectionAndSS_Rel:lt_Send_RRC_ConnectionRelease LINE 9
- Message Structure:
RLC_UM_DATA_IND
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. IntegrityResult
. uM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "10110011101011111111101100111000"
. . . . (IntegerType)rrc_MessageSequenceNumber = 1
. . . UL_DCCH_MessageType
. . . . RRCConnectionReleaseComplete
. . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . FailureCauseWithProtErr
. . . . . laterNonCriticalExtensions
. . . . . . (BitStringType)rrcConnectionReleaseComplete_r3_add_ext = 0
. . . . . . nonCriticalExtensions
- Constraint:
car_RRC_ConnRelCmplUM
- BinaryMessage:
30 0c 02 01 ff 02 01 01 d9 d7 fd 9c 0c 40

- No.: 2037
- Timestamp: 20:28:59:463_0
- RFN: 3518
- Chip: 12032
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: po_ConnectionAndSS_Rel:lt_Send_RRC_ConnectionRelease LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2040
- Timestamp: 20:28:59:464_2
- RFN: 3518
- Chip: 16896
- Event: Start Timer
- Source: po_ConnectionAndSS_Rel:lt_RptRcvConnRel LINE 1
- Message Structure:
no details available
- Constraint:
t_Dly (5000 Ms)
- BinaryMessage:

- No.: 2044
- Timestamp: 20:28:59:621_0
- RFN: 3534
- Chip: 6656
- Event: Receive
- PCO: UM
- Message: RLC_UM_DATA_IND
- Source: po_ConnectionAndSS_Rel:lt_RptRcvConnRel LINE 4
- Message Structure:
RLC_UM_DATA_IND
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. IntegrityResult
. uM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00111001011111110001011000001001"
. . . . (IntegerType)rrc_MessageSequenceNumber = 2
. . . UL_DCCH_MessageType
. . . . RRCConnectionReleaseComplete
. . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . FailureCauseWithProtErr
. . . . . laterNonCriticalExtensions
. . . . . . (BitStringType)rrcConnectionReleaseComplete_r3_add_ext = 0
. . . . . . nonCriticalExtensions
- Constraint:
car_RRC_ConnRelCmplUM
- BinaryMessage:
30 0c 02 01 ff 02 01 01 9c bf 8b 04 94 40

- No.: 2045
- Timestamp: 20:28:59:622_0
- RFN: 3534
- Chip: 10496
- Event: Cancel Timer
- Source: po_ConnectionAndSS_Rel:lt_RptRcvConnRel LINE 4
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 2046
- Timestamp: 20:28:59:622_1
- RFN: 3534
- Chip: 11520
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: po_ConnectionAndSS_Rel:lt_RptRcvConnRel LINE 4
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2062
- Timestamp: 20:28:59:629_0
- RFN: 3534
- Chip: 36608
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 01 0a 01 00 05 00

- No.: 2066
- Timestamp: 20:28:59:639_0
- RFN: 3535
- Chip: 32256
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 2069
- Timestamp: 20:28:59:642_0
- RFN: 3536
- Chip: 5376
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 02 0a 01 00 05 00

- No.: 2073
- Timestamp: 20:28:59:652_0
- RFN: 3537
- Chip: 5632
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 2076
- Timestamp: 20:28:59:655_0
- RFN: 3537
- Chip: 16896
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 03 0a 01 00 05 00

- No.: 2080
- Timestamp: 20:28:59:662_0
- RFN: 3538
- Chip: 6656
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 2083
- Timestamp: 20:28:59:665_0
- RFN: 3538
- Chip: 17664
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 04 0a 01 00 05 00

- No.: 2087
- Timestamp: 20:28:59:672_0
- RFN: 3539
- Chip: 5888
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 2093
- Timestamp: 20:28:59:676_0
- RFN: 3539
- Chip: 20480
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = -10
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 f6 0a 01 00 05 00

- No.: 2097
- Timestamp: 20:28:59:681_0
- RFN: 3540
- Chip: 4608
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = -10
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 f6

- No.: 2101
- Timestamp: 20:28:59:690_0
- RFN: 3541
- Chip: 0
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_CMAC_Rel LINE 1
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
. (RatType)ratType = 0
. configMessage
- Constraint:
cas_MAC_Rel
- BinaryMessage:
30 0b 02 01 ff 02 01 1a 0a 01 00 05 00

- No.: 2105
- Timestamp: 20:28:59:698_0
- RFN: 3541
- Chip: 30720
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_CMAC_Rel LINE 2
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 1a

- No.: 2108
- Timestamp: 20:28:59:705_0
- RFN: 3542
- Chip: 17152
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_CMAC_Rel LINE 1
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
. (RatType)ratType = 0
. configMessage
- Constraint:
cas_MAC_Rel
- BinaryMessage:
30 0b 02 01 ff 02 01 14 0a 01 00 05 00

- No.: 2112
- Timestamp: 20:28:59:710_0
- RFN: 3542
- Chip: 36608
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_CMAC_Rel LINE 2
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 14

- No.: 2115
- Timestamp: 20:28:59:712_0
- RFN: 3543
- Chip: 8448
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Release_REQ
- Source: ts_CPHY_TrChRel LINE 1
- Message Structure:
CPHY_TrCH_Release_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
ca_PHY_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 1a

- No.: 2119
- Timestamp: 20:28:59:719_0
- RFN: 3543
- Chip: 34048
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Release_CNF
- Source: ts_CPHY_TrChRel LINE 2
- Message Structure:
CPHY_TrCH_Release_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
ca_PHY_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 1a

- No.: 2122
- Timestamp: 20:28:59:722_0
- RFN: 3544
- Chip: 5888
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Release_REQ
- Source: ts_CPHY_TrChRel LINE 1
- Message Structure:
CPHY_TrCH_Release_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_PHY_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 2127
- Timestamp: 20:28:59:728_0
- RFN: 3544
- Chip: 32000
- Event: Receive
- PCO: CPHY
- Message: CPHY_Out_of_Sync_IND
- Source: SS_Def LINE 5
- Message Structure:
CPHY_Out_of_Sync_IND
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_OutOfSyncInd
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 2128
- Timestamp: 20:28:59:729_0
- RFN: 3544
- Chip: 34816
- Event: Default
- Source: SS_Def LINE 0
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2129
- Timestamp: 20:28:59:729_1
- RFN: 3544
- Chip: 35584
- Event: Default
- Source: ts_CPHY_TrChRel LINE 2
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2134
- Timestamp: 20:28:59:750_0
- RFN: 3546
- Chip: 37888
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Release_CNF
- Source: ts_CPHY_TrChRel LINE 2
- Message Structure:
CPHY_TrCH_Release_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_PHY_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 2137
- Timestamp: 20:28:59:753_0
- RFN: 3547
- Chip: 9984
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 1a

- No.: 2141
- Timestamp: 20:28:59:760_0
- RFN: 3548
- Chip: 256
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 1a

- No.: 2144
- Timestamp: 20:28:59:763_0
- RFN: 3548
- Chip: 10752
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 2148
- Timestamp: 20:28:59:789_0
- RFN: 3550
- Chip: 34304
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 2153
- Timestamp: 20:28:59:792_0
- RFN: 3551
- Chip: 7936
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 00 02 01 00 0a 01 00 05 00

- No.: 2157
- Timestamp: 20:28:59:799_0
- RFN: 3551
- Chip: 33792
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 00

- No.: 2160
- Timestamp: 20:28:59:803_0
- RFN: 3552
- Chip: 12032
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_CMAC_Rel LINE 1
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 8
. (RatType)ratType = 0
. configMessage
- Constraint:
cas_MAC_Rel
- BinaryMessage:
30 0b 02 01 00 02 01 08 0a 01 00 05 00

- No.: 2164
- Timestamp: 20:28:59:808_0
- RFN: 3552
- Chip: 29696
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_CMAC_Rel LINE 2
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 8
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 08

- No.: 2167
- Timestamp: 20:28:59:810_0
- RFN: 3553
- Chip: 2048
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Release_REQ
- Source: ts_CPHY_TrChRel LINE 1
- Message Structure:
CPHY_TrCH_Release_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 8
- Constraint:
ca_PHY_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 08

- No.: 2171
- Timestamp: 20:28:59:838_0
- RFN: 3555
- Chip: 33024
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Release_CNF
- Source: ts_CPHY_TrChRel LINE 2
- Message Structure:
CPHY_TrCH_Release_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 8
- Constraint:
ca_PHY_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 08

- No.: 2174
- Timestamp: 20:28:59:841_0
- RFN: 3556
- Chip: 5120
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 7
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 07

- No.: 2178
- Timestamp: 20:28:59:847_0
- RFN: 3556
- Chip: 29696
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 7
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 07

- No.: 2181
- Timestamp: 20:28:59:850_0
- RFN: 3557
- Chip: 1792
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 8
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 08

- No.: 2185
- Timestamp: 20:28:59:878_0
- RFN: 3559
- Chip: 32512
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 8
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 08

- No.: 2188
- Timestamp: 20:28:59:881_0
- RFN: 3560
- Chip: 5120
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -2
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 00 02 01 fe 0a 01 00 05 00

- No.: 2192
- Timestamp: 20:28:59:887_0
- RFN: 3560
- Chip: 26624
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 fe

- No.: 2195
- Timestamp: 20:28:59:890_0
- RFN: 3561
- Chip: 2560
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_CMAC_Rel LINE 1
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 5
. (RatType)ratType = 0
. configMessage
- Constraint:
cas_MAC_Rel
- BinaryMessage:
30 0b 02 01 00 02 01 05 0a 01 00 05 00

- No.: 2199
- Timestamp: 20:28:59:897_0
- RFN: 3561
- Chip: 29440
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_CMAC_Rel LINE 2
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 5
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 05

- No.: 2202
- Timestamp: 20:28:59:900_0
- RFN: 3562
- Chip: 768
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Release_REQ
- Source: ts_CPHY_TrChRel LINE 1
- Message Structure:
CPHY_TrCH_Release_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 5
- Constraint:
ca_PHY_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 05

- No.: 2206
- Timestamp: 20:28:59:907_0
- RFN: 3562
- Chip: 28416
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Release_CNF
- Source: ts_CPHY_TrChRel LINE 2
- Message Structure:
CPHY_TrCH_Release_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 5
- Constraint:
ca_PHY_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 05

- No.: 2209
- Timestamp: 20:28:59:910_0
- RFN: 3563
- Chip: 512
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 6
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 06

- No.: 2213
- Timestamp: 20:28:59:916_0
- RFN: 3563
- Chip: 24064
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 6
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 06

- No.: 2216
- Timestamp: 20:28:59:918_0
- RFN: 3563
- Chip: 34560
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 5
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 05

- No.: 2220
- Timestamp: 20:28:59:926_0
- RFN: 3564
- Chip: 25856
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 5
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 05

- No.: 2225
- Timestamp: 20:28:59:929_0
- RFN: 3565
- Chip: 256
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 00 02 01 ff 0a 01 00 05 00

- No.: 2229
- Timestamp: 20:28:59:935_0
- RFN: 3565
- Chip: 20992
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 2232
- Timestamp: 20:28:59:938_0
- RFN: 3565
- Chip: 33792
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_CMAC_Rel LINE 1
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 4
. (RatType)ratType = 0
. configMessage
- Constraint:
cas_MAC_Rel
- BinaryMessage:
30 0b 02 01 00 02 01 04 0a 01 00 05 00

- No.: 2236
- Timestamp: 20:28:59:944_0
- RFN: 3566
- Chip: 18432
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_CMAC_Rel LINE 2
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 4
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 04

- No.: 2239
- Timestamp: 20:28:59:947_0
- RFN: 3566
- Chip: 28416
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Release_REQ
- Source: ts_CPHY_TrChRel LINE 1
- Message Structure:
CPHY_TrCH_Release_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 4
- Constraint:
ca_PHY_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 04

- No.: 2243
- Timestamp: 20:28:59:955_0
- RFN: 3567
- Chip: 17920
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Release_CNF
- Source: ts_CPHY_TrChRel LINE 2
- Message Structure:
CPHY_TrCH_Release_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 4
- Constraint:
ca_PHY_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 04

- No.: 2246
- Timestamp: 20:28:59:958_0
- RFN: 3567
- Chip: 28928
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 2
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 02

- No.: 2250
- Timestamp: 20:28:59:963_0
- RFN: 3568
- Chip: 10496
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 2
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 02

- No.: 2253
- Timestamp: 20:28:59:966_0
- RFN: 3568
- Chip: 20736
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 1
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 01

- No.: 2257
- Timestamp: 20:28:59:971_0
- RFN: 3569
- Chip: 2816
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 1
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 01

- No.: 2260
- Timestamp: 20:28:59:974_0
- RFN: 3569
- Chip: 13312
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 4
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 04

- No.: 2264
- Timestamp: 20:28:59:981_0
- RFN: 3570
- Chip: 1024
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 4
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 04

- No.: 2267
- Timestamp: 20:28:59:983_0
- RFN: 3570
- Chip: 11776
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 0
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 00

- No.: 2271
- Timestamp: 20:28:59:989_0
- RFN: 3570
- Chip: 32768
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 0
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 00

- No.: 2288
- Timestamp: 20:28:59:993_2
- RFN: 3571
- Chip: 11776
- Event: Log
- PCO: VERDICT
- Message: PASS
- Source: tc_7_2_2_6 LINE 13
- Message Structure:
no details available
- Constraint:
- BinaryMessage: