- No.: 2
- Timestamp: 20:43:31:323_0
- RFN: 16956
- Chip: 512
- Event: Start Timer
- Source: tc_7_2_3_14 LINE 1
- Message Structure:
no details available
- Constraint:
t_Guard (300 Sec)
- BinaryMessage:

- No.: 88
- Timestamp: 20:43:31:391_0
- RFN: 16962
- Chip: 32512
- Event: Send
- PCO: Ut
- Message: MMI_CmdReq
- Source: ts_MMI_UE_SwitchOff LINE 1
- Message Structure:
MMI_CmdReq
. (IA5StringType)cmd[-1] = "Please switch off the UE"
- Constraint:
ca_MMI_CmdReq
- BinaryMessage:
50 6c 65 61 73 65 20 73 77 69 74 63 68 20 6f 66 66 20 20 74 68 65 20 55 45

- No.: 92
- Timestamp: 20:43:33:625_0
- RFN: 17186
- Chip: 7680
- Event: Receive
- PCO: Ut
- Message: MMI_CmdCnf
- Source: ts_MMI_UE_SwitchOff LINE 2
- Message Structure:
MMI_CmdCnf
. (BooleanType)result = TRUE
. (IA5StringType)resultString[6] = " OK "
- Constraint:
ca_MMI_CmdCnf
- BinaryMessage:
80 0d 0a 4f 4b 0d 0a

- No.: 96
- Timestamp: 20:43:33:642_0
- RFN: 17187
- Chip: 35840
- Event: Send
- PCO: CPHY
- Message: CPHY_Ini_REQ
- Source: ts_SS_CellCfg:lt_CelllsAlreadyStarted LINE 5
- Message Structure:
CPHY_Ini_REQ
. (CPHY_Ini_REQ)CPHY_Ini_REQ = 0
- Constraint:
cas_InitReqDef
- BinaryMessage:
0a 01 00

- No.: 100
- Timestamp: 20:43:35:693_0
- RFN: 10
- Chip: 14080
- Event: Receive
- PCO: CPHY
- Message: CPHY_Ini_CNF
- Source: ts_SS_CellCfg:lt_CelllsAlreadyStarted LINE 6
- Message Structure:
CPHY_Ini_CNF
- Constraint:
car_IniCnf
- BinaryMessage:
30 02 05 00

- No.: 104
- Timestamp: 20:43:35:726_0
- RFN: 13
- Chip: 22528
- Event: Send
- PCO: CPHY
- Message: CPHY_Cell_Config_REQ
- Source: ts_SS_CellCfg LINE 6
- Message Structure:
CPHY_Cell_Config_REQ
. (IntegerType)cellId = 0
. (IntegerType)tcell = 0
. (IntegerType)sfnOffset = 0
. FrequencyInfo
. . modeSpecificInfo
. . . FrequencyInfoFDD
. . . . (IntegerType)uarfcn_UL = -
. . . . (IntegerType)uarfcn_DL = 10700
. (IntegerType)primaryScramblingCode_SS = 100
. CellTxPowerLevel
. (IntegerType)dLTxAttenuationLevel = 0
- Constraint:
ca_CellCfgReq
- BinaryMessage:
30 19 02 01 00 02 01 00 02 01 00 30 06 30 04 02 02 29 cc 02 01 64 05 00 02 01 00

- No.: 108
- Timestamp: 20:43:36:694_0
- RFN: 110
- Chip: 14592
- Event: Receive
- PCO: CPHY
- Message: CPHY_Cell_Config_CNF
- Source: ts_SS_CellCfg LINE 7
- Message Structure:
CPHY_Cell_Config_CNF
. (IntegerType)cellId = 0
- Constraint:
ca_CellCfgCnf
- BinaryMessage:
30 03 02 01 00

- No.: 120
- Timestamp: 20:43:36:735_0
- RFN: 114
- Chip: 22016
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 3
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 0
. (RatType)ratType = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . PrimaryCPICHInfo
. . . . (IntegerType)dl_TxPower_PCPICH = -60
. . . . (BooleanType)txdiversityIndicator = FALSE
- Constraint:
ca_pCPICH_Info
- BinaryMessage:
30 13 02 01 00 02 01 00 0a 01 00 30 08 30 06 02 01 c4 01 01 00

- No.: 121
- Timestamp: 20:43:36:742_0
- RFN: 115
- Chip: 9728
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 4
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 0
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 00

- No.: 122
- Timestamp: 20:43:36:746_0
- RFN: 115
- Chip: 24064
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 5
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 1
. (RatType)ratType = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . PrimarySCHInfo
. . . . (BooleanType)tstdIndicator = FALSE
. . . . (IntegerType)dl_TxPower = -5
- Constraint:
ca_pSCH_Info
- BinaryMessage:
30 13 02 01 00 02 01 01 0a 01 00 30 08 30 06 01 01 00 02 01 fb

- No.: 126
- Timestamp: 20:43:36:751_0
- RFN: 116
- Chip: 5376
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 6
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 1
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 01

- No.: 127
- Timestamp: 20:43:36:763_0
- RFN: 117
- Chip: 12800
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 7
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 2
. (RatType)ratType = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . SecondarySCHInfo
. . . . (BooleanType)tstdIndicator = FALSE
. . . . (IntegerType)dl_TxPower = -5
- Constraint:
ca_sSCH_Info
- BinaryMessage:
30 13 02 01 00 02 01 02 0a 01 00 30 08 30 06 01 01 00 02 01 fb

- No.: 131
- Timestamp: 20:43:36:902_0
- RFN: 131
- Chip: 9472
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 8
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 2
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 02

- No.: 132
- Timestamp: 20:43:36:906_0
- RFN: 131
- Chip: 26368
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 9
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 4
. (RatType)ratType = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . PrimaryCCPCHInfo
. . . . (BooleanType)sttd_Indicator = FALSE
. . . . (IntegerType)dl_TxPower = -2
- Constraint:
ca_pCCPCH_Info
- BinaryMessage:
30 13 02 01 00 02 01 04 0a 01 00 30 08 30 06 01 01 00 02 01 fe

- No.: 136
- Timestamp: 20:43:36:913_0
- RFN: 132
- Chip: 15104
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 10
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 4
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 04

- No.: 137
- Timestamp: 20:43:36:989_0
- RFN: 139
- Chip: 35328
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Config_REQ
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 11
- Message Structure:
CPHY_TrCH_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 4
. (RatType)ratType = 0
. CphyTrchConfigReq
. . SS_ActivationTime
. . ulconnectedTrCHList
. . TFCS
. . dlconnectedTrCHList
. . . CphyTrchConfigReq_setseq_1
. . . . (IntegerType)trchid = 11
. . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 2
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 246
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional = 0
. . . . . . (IntegerType)rateMatchingAttribute = 1
. . . . . . (CRC_Size)crc_Size = 3
. . TFCS
. . . ExplicitTFCS_Configuration
. . . . TFCS_ReconfAdd
. . . . . ctfcSize
. . . . . . ctfc2Bit
. . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . (IntegerType)ctfc2 = 0
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . fdd
. . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 11
. . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
- Constraint:
ca_BCH_InfoActNow
- BinaryMessage:
30 4c 02 01 00 02 01 04 0a 01 00 30 41 05 00 30 23 30 21 02 01 0b 0a 01 02 30 19 30 0c 30 0a 02 02 00 f6 30 02 05 00 05 00 30 09 0a 01 00 02 01 01 0a 01 03 30 18 30 30 15 30 13 02 01 00 30 0e 30 0c 30 30 03 02 01 0b 02 01 0f 02 01 00

- No.: 138
- Timestamp: 20:43:37:042_0
- RFN: 145
- Chip: 7936
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Config_CNF
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 12
- Message Structure:
CPHY_TrCH_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 4
- Constraint:
ca_TrChCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 04

- No.: 139
- Timestamp: 20:43:37:089_0
- RFN: 149
- Chip: 34560
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 13
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 4
. (RatType)ratType = 0
. configMessage
. . CmacConfigReq
. . . SS_ActivationTime
. . . UE_Info
. . . . U_RNTI
. . . . (BitStringType)c_RNTI[16] = -
. . . TrCHInfo
. . . . ulconnectedTrCHList
. . . . TFCS
. . . . dlconnectedTrCHList
. . . . . TrCHInfo_setseq_1
. . . . . . (IntegerType)trchid = 11
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 246
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional = 0
. . . . . . . . (IntegerType)rateMatchingAttribute = 1
. . . . . . . . (CRC_Size)crc_Size = 3
. . . . TFCS
. . . . . ExplicitTFCS_Configuration
. . . . . . TFCS_ReconfAdd
. . . . . . . ctfcSize
. . . . . . . . ctfc2Bit
. . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . (IntegerType)ctfc2 = 0
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 11
. . . . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . TrCH_LogCHMappingList1
. . . . ulconnectedTrCHList
. . . . dlconnectedTrCHList
. . . . . TrCH_LogCHMappingList1_setseq_1
. . . . . . (IntegerType)trchid = 11
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 2
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 0
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 1
. . . . . . . . (IntegerType)rB_Identity = -1
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_CMAC_CfgInfo
- BinaryMessage:
30 70 02 01 00 02 01 04 0a 01 00 30 65 05 00 30 00 30 3c 30 20 30 1e 02 01 0b 30 19 30 0c 30 0a 02 02 00 f6 30 02 05 00 05 00 30 09 0a 01 00 02 01 01 0a 01 03 30 18 30 30 15 30 13 02 01 00 30 0e 30 0c 30 30 03 02 01 0b 02 01 0f 02 01 00 30 21 30 1f 30 1d 02 01 0b 30 18 30 16 30 11 0a 01 00 0a 01 02 02 01 01 0a 01 00 05 00 02 01 01 02 01 ff

- No.: 143
- Timestamp: 20:43:37:101_0
- RFN: 151
- Chip: 7168
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 14
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 4
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 04

- No.: 151
- Timestamp: 20:43:37:121_0
- RFN: 153
- Chip: 5632
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_PCH_FACH_CCCH_Cfg LINE 3
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 5
. (RatType)ratType = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . SecondaryCCPCHInfo
. . . . (IntegerType)scramblingCode = 0
. . . . SF256_AndCodeNumber
. . . . . (IntegerType)sf64 = 1
. . . . (IntegerType)sCCPCHSlotFormat = 8
. . . . (IntegerType)timingOffset = 0
. . . . (PositionFixedOrFlexible)positionFixedOrFlexible = 1
. . . . (BooleanType)sttd_Indicator = FALSE
. . . . (IntegerType)dl_TxPower = -2
. . . . (IntegerType)powerOffsetOfTFCI_PO1 = 6
. . . . (IntegerType)powerOffsetOfPILOT_PO3 = 6
- Constraint:
ca_sCCPCH_Info
- BinaryMessage:
30 28 02 01 00 02 01 05 0a 01 00 30 1d 30 1b 02 01 00 02 01 01 02 01 08 02 01 00 0a 01 01 01 01 00 02 01 fe 02 01 06 02 01 06

- No.: 152
- Timestamp: 20:43:37:128_0
- RFN: 153
- Chip: 32512
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_PCH_FACH_CCCH_Cfg LINE 4
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 5
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 05

- No.: 153
- Timestamp: 20:43:37:153_0
- RFN: 156
- Chip: 14848
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Config_REQ
- Source: ts_SS_PCH_FACH_CCCH_Cfg LINE 5
- Message Structure:
CPHY_TrCH_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 5
. (RatType)ratType = 0
. CphyTrchConfigReq
. . SS_ActivationTime
. . ulconnectedTrCHList
. . TFCS
. . dlconnectedTrCHList
. . . CphyTrchConfigReq_setseq_1
. . . . (IntegerType)trchid = 12
. . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 3
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 240
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional = 0
. . . . . . (IntegerType)rateMatchingAttribute = 230
. . . . . . (CRC_Size)crc_Size = 3
. . . CphyTrchConfigReq_setseq_1
. . . . (IntegerType)trchid = 13
. . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 1
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 168
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . (IntegerType)small = 2
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional = 0
. . . . . . (IntegerType)rateMatchingAttribute = 220
. . . . . . (CRC_Size)crc_Size = 3
. . . CphyTrchConfigReq_setseq_1
. . . . (IntegerType)trchid = 14
. . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 1
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 360
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . (IntegerType)rateMatchingAttribute = 130
. . . . . . (CRC_Size)crc_Size = 3
. . TFCS
. . . ExplicitTFCS_Configuration
. . . . TFCS_ReconfAdd
. . . . . ctfcSize
. . . . . . ctfc4Bit
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 0
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 1
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 2
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 3
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 4
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 5
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 6
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 8
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . fdd
. . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 11
. . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
- Constraint:
ca_PCH_2_FACH_InfoActNow
- BinaryMessage:
30 81 e4 02 01 00 02 01 05 0a 01 00 30 81 d8 05 00 30 74 30 24 02 01 0c 0a 01 03 30 1c 30 0e 30 0c 02 02 00 f0 30 04 05 00 05 00 05 00 30 0a 0a 01 00 02 02 00 e6 0a 01 03 30 27 02 01 0d 0a 01 01 30 1f 30 11 30 0f 02 02 00 a8 30 07 05 00 05 00 02 01 02 05 00 30 0a 0a 01 00 02 02 00 dc 0a 01 03 30 23 02 01 0e 0a 01 01 30 1b 30 0e 30 0c 02 02 01 68 30 04 05 00 05 00 05 00 30 09 05 00 02 02 00 82 0a 01 03 30 5e 30 30 5b 30 08 02 01 00 30 03 02 01 00 30 08 02 01 01 30 03 02 01 00 30 08 02 01 02 30 03 02 01 00 30 08 02 01 03 30 03 02 01 00 30 08 02 01 04 30 03 02 01 00 30 08 02 01 05 30 03 02 01 00 30 08 02 01 06 30 03 02 01 00 30 13 02 01 08 30 0e 30 0c 30 30 03 02 01 0b 02 01 0f 02 01 00

- No.: 157
- Timestamp: 20:43:37:165_0
- RFN: 157
- Chip: 20736
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Config_CNF
- Source: ts_SS_PCH_FACH_CCCH_Cfg LINE 6
- Message Structure:
CPHY_TrCH_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 5
- Constraint:
ca_TrChCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 05

- No.: 158
- Timestamp: 20:43:37:204_0
- RFN: 161
- Chip: 18688
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_SS_PCH_FACH_CCCH_Cfg LINE 7
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 5
. (RatType)ratType = 0
. configMessage
. . CmacConfigReq
. . . SS_ActivationTime
. . . UE_Info
. . . . U_RNTI
. . . . (BitStringType)c_RNTI[16] = -
. . . TrCHInfo
. . . . ulconnectedTrCHList
. . . . TFCS
. . . . dlconnectedTrCHList
. . . . . TrCHInfo_setseq_1
. . . . . . (IntegerType)trchid = 12
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 240
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional = 0
. . . . . . . . (IntegerType)rateMatchingAttribute = 230
. . . . . . . . (CRC_Size)crc_Size = 3
. . . . . TrCHInfo_setseq_1
. . . . . . (IntegerType)trchid = 13
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 168
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . (IntegerType)small = 2
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional = 0
. . . . . . . . (IntegerType)rateMatchingAttribute = 220
. . . . . . . . (CRC_Size)crc_Size = 3
. . . . . TrCHInfo_setseq_1
. . . . . . (IntegerType)trchid = 14
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 360
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . (IntegerType)rateMatchingAttribute = 130
. . . . . . . . (CRC_Size)crc_Size = 3
. . . . TFCS
. . . . . ExplicitTFCS_Configuration
. . . . . . TFCS_ReconfAdd
. . . . . . . ctfcSize
. . . . . . . . ctfc4Bit
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 0
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 1
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 2
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 3
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 4
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 5
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 6
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 8
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 11
. . . . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . TrCH_LogCHMappingList1
. . . . ulconnectedTrCHList
. . . . dlconnectedTrCHList
. . . . . TrCH_LogCHMappingList1_setseq_1
. . . . . . (IntegerType)trchid = 12
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 3
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 1
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 1
. . . . . . . . (IntegerType)rB_Identity = -2
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . TrCH_LogCHMappingList1_setseq_1
. . . . . . (IntegerType)trchid = 13
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 1
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 5
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 2
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 1
. . . . . . . . (IntegerType)rB_Identity = 0
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_CMAC_CfgInfo
- BinaryMessage:
30 82 01 23 02 01 00 02 01 05 0a 01 00 30 82 01 16 05 00 30 00 30 81 cd 30 6b 30 21 02 01 0c 30 1c 30 0e 30 0c 02 02 00 f0 30 04 05 00 05 00 05 00 30 0a 0a 01 00 02 02 00 e6 0a 01 03 30 24 02 01 0d 30 1f 30 11 30 0f 02 02 00 a8 30 07 05 00 05 00 02 01 02 05 00 30 0a 0a 01 00 02 02 00 dc 0a 01 03 30 20 02 01 0e 30 1b 30 0e 30 0c 02 02 01 68 30 04 05 00 05 00 05 00 30 09 05 00 02 02 00 82 0a 01 03 30 5e 30 30 5b 30 08 02 01 00 30 03 02 01 00 30 08 02 01 01 30 03 02 01 00 30 08 02 01 02 30 03 02 01 00 30 08 02 01 03 30 03 02 01 00 30 08 02 01 04 30 03 02 01 00 30 08 02 01 05 30 03 02 01 00 30 08 02 01 06 30 03 02 01 00 30 13 02 01 08 30 0e 30 0c 30 30 03 02 01 0b 02 01 0f 02 01 00 30 40 30 3e 30 1d 02 01 0c 30 18 30 16 30 11 0a 01 00 0a 01 03 02 01 01 0a 01 01 05 00 02 01 01 02 01 fe 30 1d 02 01 0d 30 18 30 16 30 11 0a 01 00 0a 01 01 02 01 05 0a 01 02 05 00 02 01 01 02 01 00

- No.: 162
- Timestamp: 20:43:37:249_0
- RFN: 165
- Chip: 36864
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_SS_PCH_FACH_CCCH_Cfg LINE 8
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 5
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 05

- No.: 163
- Timestamp: 20:43:37:264_0
- RFN: 167
- Chip: 15360
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_PCH_FACH_CCCH_Cfg LINE 9
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 6
. (RatType)ratType = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . PICHInfo
. . . . PICH_Info
. . . . . fdd
. . . . . . (IntegerType)channelisationCode256 = 2
. . . . . . (PI_CountPerFrame)pi_CountPerFrame = 0
. . . . . . (BooleanType)sttd_Indicator = FALSE
. . . . (IntegerType)dl_TxPower = -5
- Constraint:
ca_PICH_Info
- BinaryMessage:
30 1c 02 01 00 02 01 06 0a 01 00 30 11 30 0f 30 30 09 02 01 02 0a 01 00 01 01 00 02 01 fb

- No.: 167
- Timestamp: 20:43:37:270_0
- RFN: 168
- Chip: 1280
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_PCH_FACH_CCCH_Cfg LINE 10
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 6
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 06

- No.: 175
- Timestamp: 20:43:37:289_0
- RFN: 169
- Chip: 33024
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_RACH_CCCH_Cfg LINE 3
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 7
. (RatType)ratType = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . AICHInfo
. . . . AICH_Info
. . . . . (IntegerType)channelisationCode256 = 3
. . . . . (BooleanType)sttd_Indicator = FALSE
. . . . . (AICH_TransmissionTiming)aich_TransmissionTiming = 0
. . . . (IntegerType)dl_TxPower = -5
- Constraint:
ca_AichInfo
- BinaryMessage:
30 1b 02 01 00 02 01 07 0a 01 00 30 10 30 0e 30 09 02 01 03 01 01 00 0a 01 00 02 01 fb

- No.: 176
- Timestamp: 20:43:37:300_0
- RFN: 170
- Chip: 38144
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_RACH_CCCH_Cfg LINE 4
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 7
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 07

- No.: 177
- Timestamp: 20:43:37:304_0
- RFN: 171
- Chip: 17152
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_RACH_CCCH_Cfg LINE 5
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 8
. (RatType)ratType = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . PRACHInfo
. . . . fdd_tdd
. . . . . fdd
. . . . . . (BitStringType)preambleSignature[16] = "0000000011111111"
. . . . . . (SF_PRACH)spreadingFactorForDataPart = 1
. . . . . . (IntegerType)preambleScramblingCode = 0
. . . . . . (PuncturingLimit)puncturingLimit = 15
. . . . . . (BitStringType)accessSlot[12] = "111111111111"
- Constraint:
ca_PRACH_Info
- BinaryMessage:
30 23 02 01 00 02 01 08 0a 01 00 30 18 30 16 30 30 13 03 03 00 00 ff 0a 01 01 02 01 00 0a 01 0f 03 03 04 ff f0

- No.: 181
- Timestamp: 20:43:37:313_0
- RFN: 172
- Chip: 11264
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_RACH_CCCH_Cfg LINE 6
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 8
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 08

- No.: 182
- Timestamp: 20:43:37:323_0
- RFN: 173
- Chip: 13312
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Config_REQ
- Source: ts_SS_RACH_CCCH_Cfg LINE 7
- Message Structure:
CPHY_TrCH_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 8
. (RatType)ratType = 0
. CphyTrchConfigReq
. . SS_ActivationTime
. . ulconnectedTrCHList
. . . CphyTrchConfigReq_setseq_0
. . . . (IntegerType)trchid = 15
. . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 1
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 168
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 360
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional = 0
. . . . . . (IntegerType)rateMatchingAttribute = 150
. . . . . . (CRC_Size)crc_Size = 3
. . TFCS
. . . ExplicitTFCS_Configuration
. . . . TFCS_ReconfAdd
. . . . . ctfcSize
. . . . . . ctfc2Bit
. . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . (IntegerType)ctfc2 = 0
. . . . . . . . PowerOffsetInformation
. . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . (IntegerType)ctfc2 = 1
. . . . . . . . PowerOffsetInformation
. . dlconnectedTrCHList
. . TFCS
- Constraint:
cab_RACH_InfoActNow
- BinaryMessage:
30 4e 02 01 00 02 01 08 0a 01 00 30 43 05 00 30 30 30 2e 02 01 0f 0a 01 01 30 26 30 18 30 0a 02 02 00 a8 30 02 05 00 05 00 30 0a 02 02 01 68 30 02 05 00 05 00 30 0a 0a 01 00 02 02 00 96 0a 01 03 30 0d 30 30 0a 30 03 02 01 00 30 03 02 01 01

- No.: 186
- Timestamp: 20:43:37:331_0
- RFN: 174
- Chip: 6400
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Config_CNF
- Source: ts_SS_RACH_CCCH_Cfg LINE 8
- Message Structure:
CPHY_TrCH_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 8
- Constraint:
ca_TrChCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 08

- No.: 187
- Timestamp: 20:43:37:358_0
- RFN: 176
- Chip: 33024
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_SS_RACH_CCCH_Cfg LINE 9
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 8
. (RatType)ratType = 0
. configMessage
. . CmacConfigReq
. . . SS_ActivationTime
. . . UE_Info
. . . . U_RNTI
. . . . (BitStringType)c_RNTI[16] = -
. . . TrCHInfo
. . . . ulconnectedTrCHList
. . . . . TrCHInfo_setseq_0
. . . . . . (IntegerType)trchid = 15
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 168
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 360
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional = 0
. . . . . . . . (IntegerType)rateMatchingAttribute = 150
. . . . . . . . (CRC_Size)crc_Size = 3
. . . . TFCS
. . . . . ExplicitTFCS_Configuration
. . . . . . TFCS_ReconfAdd
. . . . . . . ctfcSize
. . . . . . . . ctfc2Bit
. . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . (IntegerType)ctfc2 = 0
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . (IntegerType)ctfc2 = 1
. . . . . . . . . . PowerOffsetInformation
. . . . dlconnectedTrCHList
. . . . TFCS
. . . TrCH_LogCHMappingList1
. . . . ulconnectedTrCHList
. . . . . TrCH_LogCHMappingList1_setseq_0
. . . . . . (IntegerType)trchid = 15
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 1
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 5
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 2
. . . . . . . . (IntegerType)rB_Identity = 0
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . dlconnectedTrCHList
- Constraint:
ca_CMAC_CfgInfo
- BinaryMessage:
30 6d 02 01 00 02 01 08 0a 01 00 30 62 05 00 30 00 30 3e 30 2d 30 2b 02 01 0f 30 26 30 18 30 0a 02 02 00 a8 30 02 05 00 05 00 30 0a 02 02 01 68 30 02 05 00 05 00 30 0a 0a 01 00 02 02 00 96 0a 01 03 30 0d 30 30 0a 30 03 02 01 00 30 03 02 01 01 30 1c 30 1a 30 18 02 01 0f 30 13 30 11 30 0c 0a 01 00 0a 01 01 02 01 05 0a 01 02 02 01 00

- No.: 191
- Timestamp: 20:43:37:366_0
- RFN: 177
- Chip: 24832
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_SS_RACH_CCCH_Cfg LINE 10
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 8
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 08

- No.: 228
- Timestamp: 20:43:37:422_0
- RFN: 183
- Chip: 9472
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_1DCH_DCCH_Cfg LINE 4
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
. (RatType)ratType = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . DPCHInfo
. . . . UL_DPCH_Info
. . . . DL_DPCHInfo
. . . . . DL_CommonInformation
. . . . . . DL_DPCH_InfoCommon
. . . . . . . cfnHandling
. . . . . . . . initialise
. . . . . . . . . (IntegerType)cfntargetsfnframeoffset = -
. . . . . . . modeSpecificInfo
. . . . . . . . fdd
. . . . . . . . . DL_DPCH_PowerControlInfo
. . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . fdd
. . . . . . . . . . . . (DPC_Mode)dpc_Mode = 0
. . . . . . . . . (IntegerType)powerOffsetPilot_pdpdch = 0
. . . . . . . . . Dl_rate_matching_restriction
. . . . . . . . . SF512_AndPilot
. . . . . . . . . . (PilotBits128)sfd128 = 0
. . . . . . . . . (PositionFixedOrFlexible)positionFixedOrFlexible = 0
. . . . . . . . . (BooleanType)tfci_Existence = FALSE
. . . . . . modeSpecificInfo
. . . . . . . fdd
. . . . . . . . (IntegerType)defaultDPCH_OffsetValue = 0
. . . . . . . . DPCH_CompressedModeInfo
. . . . . . . . (TX_DiversityMode)tx_DiversityMode = 0
. . . . . . . . SSDT_Information
. . . . . DL_DPCH_InfoPerRL
. . . . . . fdd
. . . . . . . (PCPICH_UsageForChannelEst)pCPICH_UsageForChannelEst = 0
. . . . . . . (IntegerType)dpch_FrameOffset = 0
. . . . . . . SecondaryCPICH_Info
. . . . . . . DL_ChannelisationCodeList
. . . . . . . . DL_ChannelisationCode
. . . . . . . . . (IntegerType)secondaryScramblingCode = 1
. . . . . . . . . SF512_AndCodeNumber
. . . . . . . . . . (IntegerType)sf128 = 0
. . . . . . . . . (ScramblingCodeChange)scramblingCodeChange = -
. . . . . . . (IntegerType)tpc_CombinationIndex = 0
. . . . . . . (SSDT_CellIdentity)ssdt_CellIdentity = -
. . . . . . . (ClosedLoopTimingAdjMode)closedLoopTimingAdjMode = -
. . . . . (IntegerType)powerOffsetOfTFCI_PO1 = 0
. . . . . (IntegerType)powerOffsetOfTPC_PO2 = 0
. . . . . (IntegerType)powerOffsetOfPILOT_PO3 = 0
. . . . . (IntegerType)dl_TxPower = -5
. . . . . (IntegerType)dl_TxPowerMax = 15
. . . . . (IntegerType)dl_TxPowerMin = -35
- Constraint:
ca_DL_DPCH_Info
- BinaryMessage:
30 5e 02 01 00 02 01 1a 0a 01 00 30 53 30 51 30 4f 30 25 30 1a 30 30 00 30 30 14 30 06 30 30 03 0a 01 00 02 01 00 0a 01 00 0a 01 00 01 01 00 30 30 06 02 01 00 0a 01 00 30 30 13 0a 01 00 02 01 00 30 08 30 06 02 01 01 02 01 00 02 01 00 02 01 00 02 01 00 02 01 00 02 01 fb 02 01 0f 02 01 dd

- No.: 229
- Timestamp: 20:43:37:452_0
- RFN: 186
- Chip: 9216
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_1DCH_DCCH_Cfg LINE 5
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 1a

- No.: 230
- Timestamp: 20:43:37:471_0
- RFN: 188
- Chip: 6912
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Config_REQ
- Source: ts_SS_1DCH_DCCH_Cfg LINE 6
- Message Structure:
CPHY_TrCH_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
. (RatType)ratType = 0
. CphyTrchConfigReq
. . SS_ActivationTime
. . ulconnectedTrCHList
. . TFCS
. . dlconnectedTrCHList
. . . CphyTrchConfigReq_setseq_1
. . . . (IntegerType)trchid = 10
. . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 148
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional = 1
. . . . . . (IntegerType)rateMatchingAttribute = 192
. . . . . . (CRC_Size)crc_Size = 3
. . TFCS
. . . ExplicitTFCS_Configuration
. . . . TFCS_ReconfAdd
. . . . . ctfcSize
. . . . . . ctfc2Bit
. . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . (IntegerType)ctfc2 = 0
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . (IntegerType)ctfc2 = 1
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . fdd
. . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 11
. . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
- Constraint:
ca_DCH_148_TTI_10_DL_InfoActNow
- BinaryMessage:
30 59 02 01 00 02 01 1a 0a 01 00 30 4e 05 00 30 26 30 24 02 01 0a 0a 01 00 30 1c 30 0e 30 0c 02 02 00 94 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 c0 0a 01 03 30 22 30 30 1f 30 08 02 01 00 30 03 02 01 00 30 13 02 01 01 30 0e 30 0c 30 30 03 02 01 0b 02 01 0f 02 01 00

- No.: 234
- Timestamp: 20:43:37:479_0
- RFN: 188
- Chip: 37120
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Config_CNF
- Source: ts_SS_1DCH_DCCH_Cfg LINE 7
- Message Structure:
CPHY_TrCH_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
ca_TrChCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 1a

- No.: 235
- Timestamp: 20:43:37:512_0
- RFN: 192
- Chip: 11008
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_SS_1DCH_DCCH_Cfg LINE 8
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
. (RatType)ratType = 0
. configMessage
. . CmacConfigReq
. . . SS_ActivationTime
. . . UE_Info
. . . . U_RNTI
. . . . (BitStringType)c_RNTI[16] = -
. . . TrCHInfo
. . . . ulconnectedTrCHList
. . . . TFCS
. . . . dlconnectedTrCHList
. . . . . TrCHInfo_setseq_1
. . . . . . (IntegerType)trchid = 10
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 148
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . (IntegerType)rateMatchingAttribute = 192
. . . . . . . . (CRC_Size)crc_Size = 3
. . . . TFCS
. . . . . ExplicitTFCS_Configuration
. . . . . . TFCS_ReconfAdd
. . . . . . . ctfcSize
. . . . . . . . ctfc2Bit
. . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . (IntegerType)ctfc2 = 0
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . (IntegerType)ctfc2 = 1
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 11
. . . . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . TrCH_LogCHMappingList1
. . . . ulconnectedTrCHList
. . . . dlconnectedTrCHList
. . . . . TrCH_LogCHMappingList1_setseq_1
. . . . . . (IntegerType)trchid = 10
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 1
. . . . . . . . (IntegerType)rB_Identity = 1
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 2
. . . . . . . . (IntegerType)rB_Identity = 2
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 3
. . . . . . . . (IntegerType)rB_Identity = 3
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 4
. . . . . . . . (IntegerType)rB_Identity = 4
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_CMAC_CfgInfo
- BinaryMessage:
30 81 c6 02 01 ff 02 01 1a 0a 01 00 30 81 ba 05 00 30 00 30 49 30 23 30 21 02 01 0a 30 1c 30 0e 30 0c 02 02 00 94 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 c0 0a 01 03 30 22 30 30 1f 30 08 02 01 00 30 03 02 01 00 30 13 02 01 01 30 0e 30 0c 30 30 03 02 01 0b 02 01 0f 02 01 00 30 69 30 67 30 65 02 01 0a 30 60 30 16 30 11 0a 01 00 0a 01 00 02 01 01 0a 01 04 05 00 02 01 01 02 01 01 30 16 30 11 0a 01 00 0a 01 00 02 01 02 0a 01 04 05 00 02 01 02 02 01 02 30 16 30 11 0a 01 00 0a 01 00 02 01 03 0a 01 04 05 00 02 01 03 02 01 03 30 16 30 11 0a 01 00 0a 01 00 02 01 04 0a 01 04 05 00 02 01 04 02 01 04

- No.: 239
- Timestamp: 20:43:37:529_0
- RFN: 193
- Chip: 35840
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_SS_1DCH_DCCH_Cfg LINE 9
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 1a

- No.: 240
- Timestamp: 20:43:37:540_0
- RFN: 195
- Chip: 4096
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_1DCH_DCCH_Cfg LINE 10
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
. (RatType)ratType = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . DPCHInfo
. . . . UL_DPCH_Info
. . . . . UL_DPCH_PowerControlInfo
. . . . . . fdd
. . . . . . . (IntegerType)dpcch_PowerOffset = -40
. . . . . . . (IntegerType)pc_Preamble = 1
. . . . . . . (IntegerType)sRB_delay = 7
. . . . . . . PowerControlAlgorithm
. . . . . . . . (IntegerType)algorithm1 = 1
. . . . . modeSpecificInfo
. . . . . . fdd
. . . . . . . (ScramblingCodeType)scramblingCodeType = 1
. . . . . . . (IntegerType)scramblingCode = 0
. . . . . . . (IntegerType)numberOfDPDCH = -
. . . . . . . (SpreadingFactor)spreadingFactor = 4
. . . . . . . (BooleanType)tfci_Existence = TRUE
. . . . . . . (IntegerType)numberOfFBI_Bits = -
. . . . . . . (PuncturingLimit)puncturingLimit = 15
. . . . DL_DPCHInfo
- Constraint:
ca_UL_DPCH_Info
- BinaryMessage:
30 30 02 01 00 02 01 14 0a 01 00 30 25 30 23 30 21 30 30 0c 02 01 d8 02 01 01 02 01 07 02 01 01 30 30 0f 0a 01 01 02 01 00 0a 01 04 01 01 ff 0a 01 0f

- No.: 241
- Timestamp: 20:43:37:550_0
- RFN: 196
- Chip: 2048
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_1DCH_DCCH_Cfg LINE 11
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 242
- Timestamp: 20:43:37:559_0
- RFN: 197
- Chip: 256
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Config_REQ
- Source: ts_SS_1DCH_DCCH_Cfg LINE 12
- Message Structure:
CPHY_TrCH_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
. (RatType)ratType = 0
. CphyTrchConfigReq
. . SS_ActivationTime
. . ulconnectedTrCHList
. . . CphyTrchConfigReq_setseq_0
. . . . (IntegerType)trchid = 5
. . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 148
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional = 1
. . . . . . (IntegerType)rateMatchingAttribute = 192
. . . . . . (CRC_Size)crc_Size = 3
. . TFCS
. . . ExplicitTFCS_Configuration
. . . . TFCS_ReconfAdd
. . . . . ctfcSize
. . . . . . ctfc2Bit
. . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . (IntegerType)ctfc2 = 0
. . . . . . . . PowerOffsetInformation
. . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . (IntegerType)ctfc2 = 1
. . . . . . . . PowerOffsetInformation
. . dlconnectedTrCHList
. . TFCS
- Constraint:
ca_DCH_148_TTI_10_UL_InfoActNow
- BinaryMessage:
30 44 02 01 00 02 01 14 0a 01 00 30 39 05 00 30 26 30 24 02 01 05 0a 01 00 30 1c 30 0e 30 0c 02 02 00 94 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 c0 0a 01 03 30 0d 30 30 0a 30 03 02 01 00 30 03 02 01 01

- No.: 246
- Timestamp: 20:43:37:570_0
- RFN: 198
- Chip: 5632
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Config_CNF
- Source: ts_SS_1DCH_DCCH_Cfg LINE 13
- Message Structure:
CPHY_TrCH_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_TrChCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 247
- Timestamp: 20:43:37:605_0
- RFN: 201
- Chip: 17920
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_SS_1DCH_DCCH_Cfg LINE 14
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
. (RatType)ratType = 0
. configMessage
. . CmacConfigReq
. . . SS_ActivationTime
. . . UE_Info
. . . . U_RNTI
. . . . (BitStringType)c_RNTI[16] = -
. . . TrCHInfo
. . . . ulconnectedTrCHList
. . . . . TrCHInfo_setseq_0
. . . . . . (IntegerType)trchid = 5
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 148
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . (IntegerType)rateMatchingAttribute = 192
. . . . . . . . (CRC_Size)crc_Size = 3
. . . . TFCS
. . . . . ExplicitTFCS_Configuration
. . . . . . TFCS_ReconfAdd
. . . . . . . ctfcSize
. . . . . . . . ctfc2Bit
. . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . (IntegerType)ctfc2 = 0
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . (IntegerType)ctfc2 = 1
. . . . . . . . . . PowerOffsetInformation
. . . . dlconnectedTrCHList
. . . . TFCS
. . . TrCH_LogCHMappingList1
. . . . ulconnectedTrCHList
. . . . . TrCH_LogCHMappingList1_setseq_0
. . . . . . (IntegerType)trchid = 5
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . (IntegerType)rB_Identity = 1
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . (IntegerType)rB_Identity = 2
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . (IntegerType)rB_Identity = 3
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . (IntegerType)rB_Identity = 4
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . dlconnectedTrCHList
- Constraint:
ca_CMAC_CfgInfo
- BinaryMessage:
30 81 9d 02 01 ff 02 01 14 0a 01 00 30 81 91 05 00 30 00 30 34 30 23 30 21 02 01 05 30 1c 30 0e 30 0c 02 02 00 94 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 c0 0a 01 03 30 0d 30 30 0a 30 03 02 01 00 30 03 02 01 01 30 55 30 53 30 51 02 01 05 30 4c 30 11 30 0c 0a 01 00 0a 01 00 02 01 01 0a 01 04 02 01 01 30 11 30 0c 0a 01 00 0a 01 00 02 01 02 0a 01 04 02 01 02 30 11 30 0c 0a 01 00 0a 01 00 02 01 03 0a 01 04 02 01 03 30 11 30 0c 0a 01 00 0a 01 00 02 01 04 0a 01 04 02 01 04

- No.: 251
- Timestamp: 20:43:37:620_0
- RFN: 203
- Chip: 768
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_SS_1DCH_DCCH_Cfg LINE 15
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 14

- No.: 254
- Timestamp: 20:43:37:647_0
- RFN: 205
- Chip: 28160
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB_BCCH_BCH_Cfg LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 246
. . . . . UL_RLC_Mode
. . . . . . UL_TM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . (BooleanType)segmentationIndication = FALSE
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = -
. . . . (IntegerType)dLlogicalChannelIdentity = 1
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_BCCH_Info
- BinaryMessage:
30 1d 02 01 00 02 01 ff 0a 01 00 30 12 30 0b 30 09 02 02 00 f6 30 03 01 01 00 30 03 02 01 01

- No.: 255
- Timestamp: 20:43:37:672_0
- RFN: 208
- Chip: 7168
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB_BCCH_BCH_Cfg LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 258
- Timestamp: 20:43:37:681_0
- RFN: 209
- Chip: 5888
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB_PCCH_Cfg LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -2
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 240
. . . . . UL_RLC_Mode
. . . . . . UL_TM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . (BooleanType)segmentationIndication = FALSE
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = -
. . . . (IntegerType)dLlogicalChannelIdentity = 1
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_PCCH_Info
- BinaryMessage:
30 1d 02 01 00 02 01 fe 0a 01 00 30 12 30 0b 30 09 02 02 00 f0 30 03 01 01 00 30 03 02 01 01

- No.: 262
- Timestamp: 20:43:37:687_0
- RFN: 209
- Chip: 29440
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB_PCCH_Cfg LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 fe

- No.: 265
- Timestamp: 20:43:37:703_0
- RFN: 211
- Chip: 13312
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB0_Cfg LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 152
. . . . . UL_RLC_Mode
. . . . . . UL_UM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (NoExplicitDiscard)timerBasedNoExplicit = 9
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = -
. . . . (IntegerType)dLlogicalChannelIdentity = 5
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_UM_DL_Info
- BinaryMessage:
30 1d 02 01 00 02 01 00 0a 01 00 30 12 30 0b 30 09 02 02 00 98 30 03 0a 01 09 30 03 02 01 05

- No.: 269
- Timestamp: 20:43:37:708_0
- RFN: 211
- Chip: 32000
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB0_Cfg LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 00

- No.: 270
- Timestamp: 20:43:37:714_0
- RFN: 212
- Chip: 16896
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB0_Cfg LINE 3
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_TM_RLC_Mode
. . . . . . (BooleanType)segmentationIndication = TRUE
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 166
. . . . . UL_RLC_Mode
. . . . . . UL_TM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . (BooleanType)segmentationIndication = TRUE
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = 5
. . . . (IntegerType)dLlogicalChannelIdentity = -
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_TM_UL_Info
- BinaryMessage:
30 22 02 01 00 02 01 00 0a 01 00 30 17 30 10 30 03 01 01 ff 30 09 02 02 00 a6 30 03 01 01 ff 30 03 02 01 05

- No.: 274
- Timestamp: 20:43:37:721_0
- RFN: 213
- Chip: 6400
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB0_Cfg LINE 4
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 00

- No.: 277
- Timestamp: 20:43:37:728_0
- RFN: 213
- Chip: 33280
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 136
. . . . . UL_RLC_Mode
. . . . . . UL_UM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (NoExplicitDiscard)timerBasedNoExplicit = 9
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = 1
. . . . (IntegerType)dLlogicalChannelIdentity = 1
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_UM_Info
- BinaryMessage:
30 22 02 01 ff 02 01 01 0a 01 00 30 17 30 0d 05 00 30 09 02 02 00 88 30 03 0a 01 09 30 06 02 01 01 02 01 01

- No.: 281
- Timestamp: 20:43:37:739_0
- RFN: 214
- Chip: 37376
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 282
- Timestamp: 20:43:37:755_0
- RFN: 216
- Chip: 23040
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 3
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . (TimerEPC)timerEPC = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . (TimerRST)timerRST = 9
. . . . . . . (MaxRST)max_RST = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = 2
. . . . (IntegerType)dLlogicalChannelIdentity = 2
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 02 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 27 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 02 02 01 02

- No.: 286
- Timestamp: 20:43:37:776_0
- RFN: 218
- Chip: 26880
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 4
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 287
- Timestamp: 20:43:37:785_0
- RFN: 219
- Chip: 23040
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 5
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . (TimerEPC)timerEPC = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . (TimerRST)timerRST = 9
. . . . . . . (MaxRST)max_RST = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = 3
. . . . (IntegerType)dLlogicalChannelIdentity = 3
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 03 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 27 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 03 02 01 03

- No.: 291
- Timestamp: 20:43:37:803_0
- RFN: 221
- Chip: 12544
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 6
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 292
- Timestamp: 20:43:37:812_0
- RFN: 222
- Chip: 9216
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 7
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . (TimerEPC)timerEPC = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . (TimerRST)timerRST = 9
. . . . . . . (MaxRST)max_RST = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = 4
. . . . (IntegerType)dLlogicalChannelIdentity = 4
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 04 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 27 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 04 02 01 04

- No.: 296
- Timestamp: 20:43:37:832_0
- RFN: 224
- Chip: 9984
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 8
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 337
- Timestamp: 20:43:37:900_0
- RFN: 230
- Chip: 37120
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 27
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 1b

- No.: 342
- Timestamp: 20:43:37:908_0
- RFN: 231
- Chip: 32512
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendNoSegDefSchedul LINE 2
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 343
- Timestamp: 20:43:37:932_0
- RFN: 234
- Chip: 6912
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendNoSegDefSchedul LINE 3
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 08 02 01 00 02 01 ff 00 00

- No.: 351
- Timestamp: 20:43:38:003_0
- RFN: 241
- Chip: 11520
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 11
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 0b

- No.: 356
- Timestamp: 20:43:38:008_0
- RFN: 241
- Chip: 33536
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB1 LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 357
- Timestamp: 20:43:38:021_0
- RFN: 243
- Chip: 4864
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB1 LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 1
. . . . . . . (BitStringType)sib_Data_variable[-1] = "1100010000000000000001011000100000101000000010100001000111100000000101000000000000000000000011000111010000"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 2
. . . . . . . (BitStringType)sib_Data_variable[-1] = "10000000000000000001"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 1c 02 01 00 02 01 ff 00 0e 21 69 c4 00 05 88 28 0a 11 e0 14 00 00 0c 74 04 27 00 00 20

- No.: 370
- Timestamp: 20:43:38:031_0
- RFN: 244
- Chip: 3840
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 11
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 0b

- No.: 375
- Timestamp: 20:43:38:039_0
- RFN: 244
- Chip: 37120
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB2 LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 376
- Timestamp: 20:43:38:044_0
- RFN: 245
- Chip: 17920
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB2 LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 1
. . . . . . . (BitStringType)sib_Data_variable[-1] = "1100010000000000000001011000100000101000000010100001000111100000000101000000000000000000000011000111010000"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 2
. . . . . . . (BitStringType)sib_Data_variable[-1] = "10000000000000000001"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 1c 02 01 00 02 01 ff 00 0e 21 69 c4 00 05 88 28 0a 11 e0 14 00 00 0c 74 04 27 00 00 20

- No.: 388
- Timestamp: 20:43:38:081_0
- RFN: 249
- Chip: 6144
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 10
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 0a

- No.: 393
- Timestamp: 20:43:38:088_0
- RFN: 249
- Chip: 33536
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB3 LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 394
- Timestamp: 20:43:38:093_0
- RFN: 250
- Chip: 15872
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB3 LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 7
. . . . . . . (BitStringType)sib_Data_variable[-1] = "101000101000000010000001"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 3
. . . . . . . (BitStringType)sib_Data_variable[-1] = "110000000000000000000000000000000100000011001100011000000000100100001000000100011111111111111111111111"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 1c 02 01 00 02 01 ff 00 0e 27 17 a2 80 81 1b 2e 00 00 00 02 06 63 00 48 40 8f ff ff e0

- No.: 406
- Timestamp: 20:43:38:112_0
- RFN: 252
- Chip: 10496
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 26
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 1a

- No.: 411
- Timestamp: 20:43:38:118_0
- RFN: 252
- Chip: 32000
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB4 LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 412
- Timestamp: 20:43:38:123_0
- RFN: 253
- Chip: 13056
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB4 LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 7
. . . . . . . (BitStringType)sib_Data_variable[-1] = "101000101000000010000001"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 4
. . . . . . . (BitStringType)sib_Data_variable[-1] = "1000000000000000000000000000000101100110001100000000010010000100000010001110111"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 19 02 01 00 02 01 ff 00 0e 27 17 a2 80 81 22 74 00 00 00 0b 31 80 24 20 47 70

- No.: 429
- Timestamp: 20:43:38:260_0
- RFN: 266
- Chip: 37632
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 23
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 17

- No.: 434
- Timestamp: 20:43:38:268_0
- RFN: 267
- Chip: 32768
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB5 LINE 41
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 435
- Timestamp: 20:43:38:272_0
- RFN: 268
- Chip: 8960
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB5 LINE 42
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 08 02 01 00 02 01 ff 00 00

- No.: 439
- Timestamp: 20:43:38:276_0
- RFN: 268
- Chip: 23808
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 19
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 13

- No.: 444
- Timestamp: 20:43:38:289_0
- RFN: 269
- Chip: 34048
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB5 LINE 44
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 445
- Timestamp: 20:43:38:303_0
- RFN: 271
- Chip: 14080
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB5 LINE 45
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . FirstSegment
. . . . . . (SIB_Type)sib_Type = 5
. . . . . . (IntegerType)seg_Count = 3
. . . . . . (BitStringType)sib_Data_fixed[222] = "001101010100010000111110000000001111111101000011111111111111110111010010000100001111000000101001000011000000101010100101010110000000000000001100110001011011010101111110001010111010000011111110100000111111101000001111111010"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 25 02 01 00 02 01 ff 00 02 52 35 44 3e 00 ff 43 ff fd d2 10 f0 29 0c 0a a5 58 00 0c c5 b5 7e 2b a0 fe 83 fa 0f e8

- No.: 449
- Timestamp: 20:43:38:308_0
- RFN: 271
- Chip: 31744
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 21
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 15

- No.: 454
- Timestamp: 20:43:38:318_0
- RFN: 272
- Chip: 33792
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB5 LINE 47
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 455
- Timestamp: 20:43:38:323_0
- RFN: 273
- Chip: 13824
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB5 LINE 48
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . SubsequentSegment
. . . . . . (SIB_Type)sib_Type = 5
. . . . . . (IntegerType)segmentIndex = 1
. . . . . . (BitStringType)sib_Data_fixed[222] = "000011111111010000000000000000001101011000110100010000111111010011100101000001100001000011001010000000110000001110001001000000010110000000000000100000001110000000001000100001100100001010011001000010100000000000110000000100"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 25 02 01 00 02 01 ff 00 04 50 0f f4 00 00 d6 34 43 f4 e5 06 10 ca 03 03 89 01 60 00 80 e0 08 86 42 99 0a 00 30 10

- No.: 459
- Timestamp: 20:43:38:327_0
- RFN: 273
- Chip: 30208
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 22
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 16

- No.: 464
- Timestamp: 20:43:38:339_0
- RFN: 274
- Chip: 34816
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB5 LINE 50
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 466
- Timestamp: 20:43:38:344_0
- RFN: 275
- Chip: 17408
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB5 LINE 52
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . LastSegmentShort
. . . . . . (SIB_Type)sib_Type = 5
. . . . . . (IntegerType)segmentIndex = 2
. . . . . . (BitStringType)sib_Data_variable[-1] = "010001011100101011010110100000000000011110001000011000000001011011011011011000100000000001000011000010001001010000001011011010000000010000"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 1c 02 01 00 02 01 ff 00 06 51 89 45 ca d6 80 07 88 60 16 db 62 00 43 08 94 0b 68 04 00

- No.: 483
- Timestamp: 20:43:38:364_0
- RFN: 277
- Chip: 16128
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 3
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 03

- No.: 488
- Timestamp: 20:43:38:368_0
- RFN: 277
- Chip: 34048
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB6 LINE 8
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 491
- Timestamp: 20:43:38:374_0
- RFN: 278
- Chip: 15616
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB6:lt_CompleteSIB LINE 4
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 6
. . . . . . . (BitStringType)sib_Data_variable[-1] = "0000001010010001"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 0c 02 01 00 02 01 ff 00 0e 06 0f 02 91

- No.: 496
- Timestamp: 20:43:38:378_0
- RFN: 278
- Chip: 32512
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 5
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 05

- No.: 501
- Timestamp: 20:43:38:389_0
- RFN: 279
- Chip: 35072
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB6 LINE 11
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 502
- Timestamp: 20:43:38:392_0
- RFN: 280
- Chip: 12032
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB6 LINE 12
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 08 02 01 00 02 01 ff 00 00

- No.: 506
- Timestamp: 20:43:38:396_0
- RFN: 280
- Chip: 26368
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 6
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 06

- No.: 511
- Timestamp: 20:43:38:409_0
- RFN: 281
- Chip: 36352
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB6 LINE 14
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 512
- Timestamp: 20:43:38:413_0
- RFN: 282
- Chip: 13568
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB6 LINE 15
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 08 02 01 00 02 01 ff 00 00

- No.: 516
- Timestamp: 20:43:38:417_0
- RFN: 282
- Chip: 28672
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 7
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 07

- No.: 521
- Timestamp: 20:43:38:428_0
- RFN: 283
- Chip: 34560
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB6 LINE 17
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 522
- Timestamp: 20:43:38:432_0
- RFN: 284
- Chip: 10752
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB6 LINE 18
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 08 02 01 00 02 01 ff 00 00

- No.: 530
- Timestamp: 20:43:38:446_0
- RFN: 285
- Chip: 24320
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 2
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 02

- No.: 535
- Timestamp: 20:43:38:453_0
- RFN: 286
- Chip: 14592
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB7 LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 538
- Timestamp: 20:43:38:461_0
- RFN: 287
- Chip: 7168
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB7:lt_CompleteSIB LINE 4
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 7
. . . . . . . (BitStringType)sib_Data_variable[-1] = "101000101000000010000001"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 0d 02 01 00 02 01 ff 00 0e 07 17 a2 80 81

- No.: 546
- Timestamp: 20:43:38:476_0
- RFN: 288
- Chip: 27136
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 10
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 0a

- No.: 551
- Timestamp: 20:43:38:484_0
- RFN: 289
- Chip: 19712
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB7:lt_ConcatWithSIB3 LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 552
- Timestamp: 20:43:38:491_0
- RFN: 290
- Chip: 6656
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB7:lt_ConcatWithSIB3 LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 7
. . . . . . . (BitStringType)sib_Data_variable[-1] = "101000101000000010000001"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 3
. . . . . . . (BitStringType)sib_Data_variable[-1] = "110000000000000000000000000000000100000011001100011000000000100100001000000100011111111111111111111111"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 1c 02 01 00 02 01 ff 00 0e 27 17 a2 80 81 1b 2e 00 00 00 02 06 63 00 48 40 8f ff ff e0

- No.: 560
- Timestamp: 20:43:38:542_0
- RFN: 295
- Chip: 7168
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 18
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 12

- No.: 565
- Timestamp: 20:43:38:550_0
- RFN: 296
- Chip: 1280
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB7:lt_ConcatWithSIB18 LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 566
- Timestamp: 20:43:38:557_0
- RFN: 296
- Chip: 26368
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB7:lt_ConcatWithSIB18 LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 7
. . . . . . . (BitStringType)sib_Data_variable[-1] = "101000101000000010000001"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 26
. . . . . . . (BitStringType)sib_Data_variable[-1] = "100100000001000000000001000000001"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 13 02 01 00 02 01 ff 00 0e 27 17 a2 80 81 d1 04 80 80 08 04

- No.: 574
- Timestamp: 20:43:38:579_0
- RFN: 298
- Chip: 33792
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 26
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 1a

- No.: 579
- Timestamp: 20:43:38:589_0
- RFN: 299
- Chip: 36352
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB7:lt_ConcatWithSIB4 LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 580
- Timestamp: 20:43:38:596_0
- RFN: 300
- Chip: 23040
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB7:lt_ConcatWithSIB4 LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 7
. . . . . . . (BitStringType)sib_Data_variable[-1] = "101000101000000010000001"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 4
. . . . . . . (BitStringType)sib_Data_variable[-1] = "1000000000000000000000000000000101100110001100000000010010000100000010001110111"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 19 02 01 00 02 01 ff 00 0e 27 17 a2 80 81 22 74 00 00 00 0b 31 80 24 20 47 70

- No.: 594
- Timestamp: 20:43:38:711_0
- RFN: 312
- Chip: 6912
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 31
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 1f

- No.: 599
- Timestamp: 20:43:38:718_0
- RFN: 312
- Chip: 32768
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB11 LINE 20
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 600
- Timestamp: 20:43:38:722_0
- RFN: 313
- Chip: 9728
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB11 LINE 21
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 08 02 01 00 02 01 ff 00 00

- No.: 604
- Timestamp: 20:43:38:726_0
- RFN: 313
- Chip: 24064
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 29
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 1d

- No.: 609
- Timestamp: 20:43:38:738_0
- RFN: 314
- Chip: 34816
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB11 LINE 23
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 610
- Timestamp: 20:43:38:743_0
- RFN: 315
- Chip: 14592
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB11 LINE 24
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . FirstSegment
. . . . . . (SIB_Type)sib_Type = 11
. . . . . . (IntegerType)seg_Count = 2
. . . . . . (BitStringType)sib_Data_fixed[222] = "011000001101100100010010000000001000110010000100001000010010010110101000100000100110010001010011000001011001000010100111000010111000010100001000100010001100100101010100000001001010000101001010100001100001001010001000001010"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 25 02 01 00 02 01 ff 00 02 b1 60 d9 12 00 8c 84 21 25 a8 82 64 53 05 90 a7 0b 85 08 88 c9 54 04 a1 4a 86 12 88 28

- No.: 614
- Timestamp: 20:43:38:748_0
- RFN: 315
- Chip: 32000
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 30
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 1e

- No.: 619
- Timestamp: 20:43:38:758_0
- RFN: 316
- Chip: 34048
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB11 LINE 26
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 621
- Timestamp: 20:43:38:763_0
- RFN: 317
- Chip: 15360
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB11 LINE 28
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . LastSegmentShort
. . . . . . (SIB_Type)sib_Type = 11
. . . . . . (IntegerType)segmentIndex = 1
. . . . . . (BitStringType)sib_Data_variable[-1] = "000100001100001001010010011010101000011000010010101000101100011001010100101010100001001111101000100010000001010010110000100010100001010101111000"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 1c 02 01 00 02 01 ff 00 06 b0 8f 10 c2 52 6a 86 12 a2 c6 54 aa 13 e8 88 14 b0 8a 15 78

- No.: 634
- Timestamp: 20:43:38:779_0
- RFN: 319
- Chip: 512
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 13
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 0d

- No.: 639
- Timestamp: 20:43:38:791_0
- RFN: 320
- Chip: 7424
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB12 LINE 8
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 642
- Timestamp: 20:43:38:797_0
- RFN: 320
- Chip: 28928
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB12:lt_CompleteSIB LINE 4
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 12
. . . . . . . (BitStringType)sib_Data_variable[-1] = "010000000"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 0c 02 01 00 02 01 ff 00 0e 0c 08 40 00

- No.: 647
- Timestamp: 20:43:38:801_0
- RFN: 321
- Chip: 6912
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 14
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 0e

- No.: 652
- Timestamp: 20:43:38:809_0
- RFN: 322
- Chip: 768
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB12 LINE 11
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 653
- Timestamp: 20:43:38:813_0
- RFN: 322
- Chip: 15872
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB12 LINE 12
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 08 02 01 00 02 01 ff 00 00

- No.: 657
- Timestamp: 20:43:38:817_0
- RFN: 322
- Chip: 30464
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 15
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 0f

- No.: 662
- Timestamp: 20:43:38:828_0
- RFN: 323
- Chip: 35584
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB12 LINE 14
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 663
- Timestamp: 20:43:38:833_0
- RFN: 324
- Chip: 12032
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB12 LINE 15
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 08 02 01 00 02 01 ff 00 00

- No.: 671
- Timestamp: 20:43:38:841_0
- RFN: 325
- Chip: 3840
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 18
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 12

- No.: 676
- Timestamp: 20:43:38:851_0
- RFN: 326
- Chip: 2304
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB18 LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 677
- Timestamp: 20:43:38:856_0
- RFN: 326
- Chip: 21504
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB18 LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 7
. . . . . . . (BitStringType)sib_Data_variable[-1] = "101000101000000010000001"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 26
. . . . . . . (BitStringType)sib_Data_variable[-1] = "100100000001000000000001000000001"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 13 02 01 00 02 01 ff 00 0e 27 17 a2 80 81 d1 04 80 80 08 04

- No.: 689
- Timestamp: 20:43:38:873_0
- RFN: 328
- Chip: 10752
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 4
. . (IntegerType)sg_POS = 1
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 04 02 01 01

- No.: 694
- Timestamp: 20:43:38:878_0
- RFN: 328
- Chip: 32768
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSB1_DefSchedul LINE 4
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 697
- Timestamp: 20:43:38:884_0
- RFN: 329
- Chip: 15360
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSB1_DefSchedul:lt_CompleteSIB LINE 4
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 27
. . . . . . . (BitStringType)sib_Data_variable[-1] = "10010000101010001000001100110000010010010100111000101001110100000000010110100010001101110010100010010010"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 17 02 01 00 02 01 ff 00 0e 1b 67 90 a8 83 30 49 4e 29 d0 05 a2 37 28 92

- No.: 715
- Timestamp: 20:43:38:896_0
- RFN: 330
- Chip: 24832
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 3
. . (IntegerType)sg_POS = 0
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 03 02 01 00

- No.: 720
- Timestamp: 20:43:38:901_0
- RFN: 331
- Chip: 4096
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendMIB LINE 7
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 723
- Timestamp: 20:43:38:906_0
- RFN: 331
- Chip: 25088
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendMIB:lt_CompleteSIB LINE 4
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 0
. . . . . . . (BitStringType)sib_Data_variable[-1] = "0001000000000000010000000010010110101010000100010000000000001000100010110000101000100010110001001000100010100001101000100110100010001110010010010011000100010000"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 1e 02 01 00 02 01 ff 00 0e 00 9f 10 00 40 25 aa 11 00 08 8b 0a 22 c4 88 a1 a2 68 8e 49 31 10

- No.: 738
- Timestamp: 20:43:38:915_0
- RFN: 332
- Chip: 18688
- Event: Send
- PCO: Ut
- Message: MMI_CmdReq
- Source: ts_MMI_UE_SwitchOn LINE 1
- Message Structure:
MMI_CmdReq
. (IA5StringType)cmd[-1] = "Please switch on the UE"
- Constraint:
ca_MMI_CmdReq
- BinaryMessage:
50 6c 65 61 73 65 20 73 77 69 74 63 68 20 6f 6e 20 74 68 65 20 55 45

- No.: 745
- Timestamp: 20:43:58:692_0
- RFN: 2310
- Chip: 10752
- Event: Receive
- PCO: Ut
- Message: MMI_CmdCnf
- Source: ts_MMI_UE_SwitchOn LINE 2
- Message Structure:
MMI_CmdCnf
. (BooleanType)result = TRUE
. (IA5StringType)resultString[6] = " OK "
- Constraint:
ca_MMI_CmdCnf
- BinaryMessage:
80 0d 0a 4f 4b 0d 0a

- No.: 761
- Timestamp: 20:43:58:763_0
- RFN: 2317
- Chip: 12288
- Event: Receive
- PCO: TM
- Message: RLC_TR_DATA_IND
- Source: ts_RRC_ConnEst:lt_RcvConnReq LINE 2
- Message Structure:
RLC_TR_DATA_IND
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
. tM_message
. . UL_CCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode = 0
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . UL_CCCH_MessageType
. . . . RRCConnectionRequest
. . . . . InitialUE_Identity
. . . . . . TMSI_and_LAI_GSM_MAP
. . . . . . . (BitStringType)tmsi[32] = "00010010001101000101011001111000"
. . . . . . . LAI
. . . . . . . . PLMN_Identity
. . . . . . . . . MCC
. . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . (IntegerType)_elem = 1
. . . . . . . . . MNC
. . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . (IntegerType)_elem = 1
. . . . . . . . (BitStringType)lac[16] = '0000000000000001'B
. . . . . (EstablishmentCause)establishmentCause = 12
. . . . . (ProtocolErrorIndicator)protocolErrorIndicator = 0
. . . . . MeasuredResultsOnRACH
. . . . . . currentCell
. . . . . . . modeSpecificInfo
. . . . . . . . fdd
. . . . . . . . . measurementQuantity
. . . . . . . . . . (IntegerType)cpich_Ec_N0 = 0
. . . . . v3d0NonCriticalExtensions
. . . . . . RRCConnectionRequest_v3d0ext_IEs
. . . . . . . (BitStringType)uESpecificBehaviourInformation1idle = 0
. . . . . . nonCriticalExtensions
- Constraint:
car_RRC_ConnReq
- BinaryMessage:
30 11 02 01 00 02 01 00 21 12 34 56 78 00 10 08 00 0b 00

- No.: 765
- Timestamp: 20:43:58:934_0
- RFN: 2334
- Chip: 16384
- Event: Send
- PCO: UM
- Message: RLC_UM_DATA_REQ
- Source: ts_RRC_ConnEst:lt_Send_ConnSetUp LINE 22
- Message Structure:
RLC_UM_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
. uM_message
. . DL_CCCH_Message
. . . IntegrityCheckInfo
. . . DL_CCCH_MessageType
. . . . RRCConnectionSetup
. . . . . r3
. . . . . . RRCConnectionSetup_r3_IEs
. . . . . . . InitialUE_Identity
. . . . . . . . TMSI_and_LAI_GSM_MAP
. . . . . . . . . (BitStringType)tmsi[32] = "00010010001101000101011001111000"
. . . . . . . . . LAI
. . . . . . . . . . PLMN_Identity
. . . . . . . . . . . MCC
. . . . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . . . (IntegerType)_elem = 1
. . . . . . . . . . . MNC
. . . . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . . . (IntegerType)_elem = 1
. . . . . . . . . . (BitStringType)lac[16] = '0000000000000001'B
. . . . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . . . (IntegerType)activationTime = -
. . . . . . . U_RNTI
. . . . . . . . (BitStringType)srnc_Identity[12] = "000000000001"
. . . . . . . . (BitStringType)s_RNTI[20] = "00000000000000000001"
. . . . . . . (BitStringType)new_c_RNTI[16] = -
. . . . . . . (RRC_StateIndicator)rrc_StateIndicator = 0
. . . . . . . (IntegerType)utran_DRX_CycleLengthCoeff = 9
. . . . . . . CapabilityUpdateRequirement
. . . . . . . . (BooleanType)ue_RadioCapabilityFDDUpdateRequirement = TRUE
. . . . . . . . (BooleanType)ue_RadioCapabilityTDDUpdateRequirement = FALSE
. . . . . . . . SystemSpecificCapUpdateReqList
. . . . . . . . . (SystemSpecificCapUpdateReq)_elem = 0
. . . . . . . SRB_InformationSetupList2
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_UM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 1
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 1
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . . . . . . . (TimerRST)timerRST = 9
. . . . . . . . . . . . . (MaxRST)max_RST = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 2
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 2
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . . . . . . . (TimerRST)timerRST = 9
. . . . . . . . . . . . . (MaxRST)max_RST = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 3
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 3
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . . . . . . . (TimerRST)timerRST = 9
. . . . . . . . . . . . . (MaxRST)max_RST = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 4
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 4
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . UL_CommonTransChInfo
. . . . . . . . TFC_Subset
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . TFCS
. . . . . . . . . . . ExplicitTFCS_Configuration
. . . . . . . . . . . . TFCS_ReconfAdd
. . . . . . . . . . . . . ctfcSize
. . . . . . . . . . . . . . ctfc2Bit
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . . . . . . . (IntegerType)ctfc2 = 0
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . . . . . . . (IntegerType)ctfc2 = 1
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 11
. . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . UL_AddReconfTransChInfoList
. . . . . . . . UL_AddReconfTransChInformation
. . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType = 0
. . . . . . . . . (IntegerType)transportChannelIdentity = 5
. . . . . . . . . TransportFormatSet
. . . . . . . . . . DedicatedTransChTFS
. . . . . . . . . . . tti
. . . . . . . . . . . . DedicatedDynamicTF_InfoList
. . . . . . . . . . . . . DedicatedDynamicTF_Info
. . . . . . . . . . . . . . rlc_Size
. . . . . . . . . . . . . . . BitModeRLC_SizeInfo
. . . . . . . . . . . . . . . . sizeType2
. . . . . . . . . . . . . . . . . (IntegerType)part1 = 2
. . . . . . . . . . . . . . . . . (IntegerType)part2 = -
. . . . . . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . LogicalChannelList
. . . . . . . . . . . SemistaticTF_Information
. . . . . . . . . . . . ChannelCodingType
. . . . . . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . . . . . (IntegerType)rateMatchingAttribute = 192
. . . . . . . . . . . . (CRC_Size)crc_Size = 3
. . . . . . . DL_CommonTransChInfo
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . dl_Parameters
. . . . . . . DL_AddReconfTransChInfoList
. . . . . . . . DL_AddReconfTransChInformation
. . . . . . . . . (DL_TrCH_Type)dl_TransportChannelType = 0
. . . . . . . . . (IntegerType)dl_transportChannelIdentity = 10
. . . . . . . . . tfs_SignallingMode
. . . . . . . . . . UL_TransportChannelIdentity
. . . . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType = 0
. . . . . . . . . . . (IntegerType)ul_TransportChannelIdentity = 5
. . . . . . . . . QualityTarget
. . . . . . . . . . (IntegerType)bler_QualityValue = -20
. . . . . . . . . TM_SignallingInfo
. . . . . . . FrequencyInfo
. . . . . . . (IntegerType)maxAllowedUL_TX_Power = -
. . . . . . . UL_ChannelRequirement
. . . . . . . . UL_DPCH_Info
. . . . . . . . . UL_DPCH_PowerControlInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (IntegerType)dpcch_PowerOffset = -40
. . . . . . . . . . . (IntegerType)pc_Preamble = 1
. . . . . . . . . . . (IntegerType)sRB_delay = 7
. . . . . . . . . . . PowerControlAlgorithm
. . . . . . . . . . . . (IntegerType)algorithm1 = 1
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (ScramblingCodeType)scramblingCodeType = 1
. . . . . . . . . . . (IntegerType)scramblingCode = 0
. . . . . . . . . . . (IntegerType)numberOfDPDCH = -
. . . . . . . . . . . (SpreadingFactor)spreadingFactor = 4
. . . . . . . . . . . (BooleanType)tfci_Existence = TRUE
. . . . . . . . . . . (IntegerType)numberOfFBI_Bits = -
. . . . . . . . . . . (PuncturingLimit)puncturingLimit = 15
. . . . . . . DL_CommonInformation
. . . . . . . . DL_DPCH_InfoCommon
. . . . . . . . . cfnHandling
. . . . . . . . . . initialise
. . . . . . . . . . . (IntegerType)cfntargetsfnframeoffset = -
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . DL_DPCH_PowerControlInfo
. . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . (DPC_Mode)dpc_Mode = 0
. . . . . . . . . . . (IntegerType)powerOffsetPilot_pdpdch = 0
. . . . . . . . . . . Dl_rate_matching_restriction
. . . . . . . . . . . SF512_AndPilot
. . . . . . . . . . . . (PilotBits128)sfd128 = 0
. . . . . . . . . . . (PositionFixedOrFlexible)positionFixedOrFlexible = 0
. . . . . . . . . . . (BooleanType)tfci_Existence = FALSE
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . (IntegerType)defaultDPCH_OffsetValue = 0
. . . . . . . . . . DPCH_CompressedModeInfo
. . . . . . . . . . (TX_DiversityMode)tx_DiversityMode = 0
. . . . . . . . . . SSDT_Information
. . . . . . . DL_InformationPerRL_List
. . . . . . . . DL_InformationPerRL
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . PrimaryCPICH_Info
. . . . . . . . . . . . (IntegerType)primaryScramblingCode = 100
. . . . . . . . . . . PDSCH_SHO_DCH_Info
. . . . . . . . . . . PDSCH_CodeMapping
. . . . . . . . . DL_DPCH_InfoPerRL
. . . . . . . . . . fdd
. . . . . . . . . . . (PCPICH_UsageForChannelEst)pCPICH_UsageForChannelEst = 0
. . . . . . . . . . . (IntegerType)dpch_FrameOffset = 0
. . . . . . . . . . . SecondaryCPICH_Info
. . . . . . . . . . . DL_ChannelisationCodeList
. . . . . . . . . . . . DL_ChannelisationCode
. . . . . . . . . . . . . (IntegerType)secondaryScramblingCode = 1
. . . . . . . . . . . . . SF512_AndCodeNumber
. . . . . . . . . . . . . . (IntegerType)sf128 = 0
. . . . . . . . . . . . . (ScramblingCodeChange)scramblingCodeChange = 1
. . . . . . . . . . . (IntegerType)tpc_CombinationIndex = 0
. . . . . . . . . . . (SSDT_CellIdentity)ssdt_CellIdentity = -
. . . . . . . . . . . (ClosedLoopTimingAdjMode)closedLoopTimingAdjMode = -
. . . . . . . . . SCCPCH_InfoForFACH
. . . . . . laterNonCriticalExtensions
. (BooleanType)specialLI = TRUE
- Constraint:
cas_RRC_ConnSetup
- BinaryMessage:
30 78 02 01 00 02 01 00 30 e7 22 46 8a cf 00 02 01 00 01 00 04 00 00 4d 82 69 3a 10 10 89 0d 42 00 02 81 9e 8e 46 c9 ce 7c 9c 4e 74 20 a5 12 3a 8c 00 15 13 3d 1c 8d 93 9c f9 38 9c e8 42 52 24 b5 28 00 4a 46 7a 39 1b 27 39 f2 71 39 d0 86 b4 49 ea 70 00 d4 c8 00 06 25 2b f0 02 00 08 82 23 bf 66 08 98 95 a5 47 a2 00 00 01 3f 90 0a 14 00 02 06 40 00 0c 28 08 01 01 ff

- No.: 786
- Timestamp: 20:43:59:046_2
- RFN: 2345
- Chip: 26112
- Event: Start Timer
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 3
- Message Structure:
no details available
- Constraint:
t_WaitMS (13500 Ms)
- BinaryMessage:

- No.: 791
- Timestamp: 20:43:59:208_0
- RFN: 2361
- Chip: 31488
- Event: Receive
- PCO: CPHY
- Message: CPHY_Sync_IND
- Source: RRC_Def1 LINE 13
- Message Structure:
CPHY_Sync_IND
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_SyncInd
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 792
- Timestamp: 20:43:59:209_0
- RFN: 2361
- Chip: 33280
- Event: Cancel Timer
- Source: RRC_Def1 LINE 13
- Message Structure:
no details available
- Constraint:
t_T312
- BinaryMessage:

- No.: 793
- Timestamp: 20:43:59:218_0
- RFN: 2362
- Chip: 29696
- Event: Default
- Source: RRC_Def1 LINE 0
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 794
- Timestamp: 20:43:59:218_1
- RFN: 2362
- Chip: 30464
- Event: Default
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 799
- Timestamp: 20:43:59:669_0
- RFN: 2407
- Chip: 35840
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_IND
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
RLC_AM_DATA_IND
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. IntegrityResult
. . (IntegrityStatus)integrityUsed = 0
. aM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode = 0
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . UL_DCCH_MessageType
. . . . RRCConnectionSetupComplete
. . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . STARTList
. . . . . . STARTSingle
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity = 1
. . . . . . . (BitStringType)start_Value[20] = "00000000000000000100"
. . . . . . STARTSingle
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity = 0
. . . . . . . (BitStringType)start_Value[20] = "00000000000000000010"
. . . . . UE_RadioAccessCapability
. . . . . . (AccessStratumReleaseIndicator)accessStratumReleaseIndicator = 0
. . . . . . PDCP_Capability
. . . . . . . (BooleanType)losslessSRNS_RelocationSupport = FALSE
. . . . . . . supportForRfc2507
. . . . . . RLC_Capability
. . . . . . . (TotalRLC_AM_BufferSize)totalRLC_AM_BufferSize = 2
. . . . . . . (MaximumRLC_WindowSize)maximumRLC_WindowSize = 0
. . . . . . . (MaximumAM_EntityNumberRLC_Cap)maximumAM_EntityNumber = 3
. . . . . . TransportChannelCapability
. . . . . . . DL_TransChCapability
. . . . . . . . (MaxNoBits)maxNoBitsReceived = 4
. . . . . . . . (MaxNoBits)maxConvCodeBitsReceived = 1
. . . . . . . . TurboSupport
. . . . . . . . . (MaxNoBits)supported = 4
. . . . . . . . (MaxSimultaneousTransChsDL)maxSimultaneousTransChs = 1
. . . . . . . . (IntegerType)maxSimultaneousCCTrCH_Count = 1
. . . . . . . . (MaxTransportBlocksDL)maxReceivedTransportBlocks = 2
. . . . . . . . (MaxNumberOfTFC_DL)maxNumberOfTFC = 4
. . . . . . . . (MaxNumberOfTF)maxNumberOfTF = 1
. . . . . . . UL_TransChCapability
. . . . . . . . (MaxNoBits)maxNoBitsTransmitted = 3
. . . . . . . . (MaxNoBits)maxConvCodeBitsTransmitted = 1
. . . . . . . . TurboSupport
. . . . . . . . . (MaxNoBits)supported = 3
. . . . . . . . (MaxSimultaneousTransChsUL)maxSimultaneousTransChs = 2
. . . . . . . . modeSpecificInfo
. . . . . . . . (MaxTransportBlocksUL)maxTransmittedBlocks = 2
. . . . . . . . (MaxNumberOfTFC_UL)maxNumberOfTFC = 3
. . . . . . . . (MaxNumberOfTF)maxNumberOfTF = 0
. . . . . . RF_Capability
. . . . . . . fddRF_Capability
. . . . . . . . (IntegerType)ue_PowerClass = 4
. . . . . . . . (TxRxFrequencySeparation)txRxFrequencySeparation = 0
. . . . . . . tddRF_Capability
. . . . . . . . (IntegerType)ue_PowerClass = 0
. . . . . . . . (RadioFrequencyBandTDDList)radioFrequencyTDDBandList = 0
. . . . . . . . (ChipRateCapability)chipRateCapability = 0
. . . . . . PhysicalChannelCapability
. . . . . . . fddPhysChCapability
. . . . . . . . DL_PhysChCapabilityFDD
. . . . . . . . . (IntegerType)maxNoDPCH_PDSCH_Codes = 3
. . . . . . . . . (MaxNoPhysChBitsReceived)maxNoPhysChBitsReceived = 6
. . . . . . . . . (BooleanType)supportForSF_512 = FALSE
. . . . . . . . . (BooleanType)supportOfPDSCH = FALSE
. . . . . . . . . SimultaneousSCCPCH_DPCH_Reception
. . . . . . . . UL_PhysChCapabilityFDD
. . . . . . . . . (MaxNoDPDCH_BitsTransmitted)maxNoDPDCH_BitsTransmitted = 2
. . . . . . . . . (BooleanType)supportOfPCPCH = FALSE
. . . . . . . tddPhysChCapability
. . . . . . . . DL_PhysChCapabilityTDD
. . . . . . . . . (IntegerType)maxTS_PerFrame = 0
. . . . . . . . . (IntegerType)maxPhysChPerFrame = 0
. . . . . . . . . (MinimumSF_DL)minimumSF = 0
. . . . . . . . . (BooleanType)supportOfPDSCH = FALSE
. . . . . . . . . (IntegerType)maxPhysChPerTS = 0
. . . . . . . . UL_PhysChCapabilityTDD
. . . . . . . . . (IntegerType)maxTS_PerFrame = 0
. . . . . . . . . (MaxPhysChPerTimeslot)maxPhysChPerTimeslot = 0
. . . . . . . . . (MinimumSF_UL)minimumSF = 0
. . . . . . . . . (BooleanType)supportOfPUSCH = FALSE
. . . . . . UE_MultiModeRAT_Capability
. . . . . . . MultiRAT_Capability
. . . . . . . . (BooleanType)supportOfGSM = TRUE
. . . . . . . . (BooleanType)supportOfMulticarrier = FALSE
. . . . . . . (MultiModeCapability)multiModeCapability = 1
. . . . . . SecurityCapability
. . . . . . . (BitStringType)cipheringAlgorithmCap[16] = '0000000000000011'B
. . . . . . . (BitStringType)integrityProtectionAlgorithmCap[16] = '0000000000000010'B
. . . . . . UE_Positioning_Capability
. . . . . . . (BooleanType)standaloneLocMethodsSupported = FALSE
. . . . . . . (BooleanType)ue_BasedOTDOA_Supported = FALSE
. . . . . . . (NetworkAssistedGPS_Supported)networkAssistedGPS_Supported = 3
. . . . . . . (BooleanType)supportForUE_GPS_TimingOfCellFrames = FALSE
. . . . . . . (BooleanType)supportForIPDL = FALSE
. . . . . . MeasurementCapability
. . . . . . . CompressedModeMeasCapability
. . . . . . . . (BooleanType)fdd_Measurements = TRUE
. . . . . . . . (BooleanType)tdd_Measurements = FALSE
. . . . . . . . GSM_Measurements
. . . . . . . . . (BooleanType)gsm900 = TRUE
. . . . . . . . . (BooleanType)dcs1800 = TRUE
. . . . . . . . . (BooleanType)gsm1900 = FALSE
. . . . . . . . (BooleanType)multiCarrierMeasurements = FALSE
. . . . . . . CompressedModeMeasCapability
. . . . . . . . (BooleanType)fdd_Measurements = TRUE
. . . . . . . . (BooleanType)tdd_Measurements = FALSE
. . . . . . . . GSM_Measurements
. . . . . . . . . (BooleanType)gsm900 = TRUE
. . . . . . . . . (BooleanType)dcs1800 = TRUE
. . . . . . . . . (BooleanType)gsm1900 = FALSE
. . . . . . . . (BooleanType)multiCarrierMeasurements = FALSE
. . . . . v370NonCriticalExtensions
. . . . . . RRCConnectionSetupComplete_v370ext
. . . . . . . UE_RadioAccessCapability_v370ext
. . . . . . v380NonCriticalExtensions
. . . . . . . RRCConnectionSetupComplete_v380ext_IEs
. . . . . . . . UE_RadioAccessCapability_v380ext
. . . . . . . . . UE_PositioningCapabilityExt_v380
. . . . . . . . . . (BooleanType)rx_tx_TimeDifferenceType2Capable = FALSE
. . . . . . . . DL_PhysChCapabilityFDD_v380ext
. . . . . . . . . (SupportOfDedicatedPilotsForChEstimation)supportOfDedicatedPilotsForChEstimation = 0
. . . . . . . v3a0NonCriticalExtensions
. . . . . . . . RRCConnectionSetupComplete_v3a0ext_IEs
. . . . . . . . . UE_RadioAccessCapability_v3a0ext
. . . . . . . . . . UE_PositioningCapabilityExt_v3a0
. . . . . . . . . . . (UE_PositioningCapabilityExt_v3a0_list_0)validity_CellPCH_UraPCH = 0
. . . . . . . . laterNonCriticalExtensions
. . . . . . . . . (BitStringType)rrcConnectionSetupComplete_r3_add_ext = 0
. . . . . . . . . nonCriticalExtensions
- Constraint:
car_RRC_ConnSetupCmpl
- BinaryMessage:
30 27 02 01 ff 02 01 02 0a 05 01 00 00 00 00 4a 0c 00 01 00 00 05 11 a0 d1 04 84 c6 68 46 2c 93 02 48 00 18 00 11 8f 8f 80

- No.: 800
- Timestamp: 20:43:59:718_0
- RFN: 2412
- Chip: 34304
- Event: Cancel Timer
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
t_WaitMS
- BinaryMessage:

- No.: 801
- Timestamp: 20:43:59:719_0
- RFN: 2412
- Chip: 35072
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 815
- Timestamp: 20:43:59:735_0
- RFN: 2414
- Chip: 22272
- Event: Send
- PCO: CMAC
- Message: CMAC_SecurityMode_Config_REQ
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 1
- Message Structure:
CMAC_SecurityMode_Config_REQ
. (IntegerType)cellId = 0
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity = 1
. . (BitStringType)startValue[20] = "00000000000000000100"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = -
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CMAC_SecurityModeCfgReq
- BinaryMessage:
30 0e 02 01 00 30 09 0a 01 01 03 04 04 00 00 40

- No.: 816
- Timestamp: 20:43:59:737_0
- RFN: 2414
- Chip: 28928
- Event: Receive
- PCO: CMAC
- Message: CMAC_SecurityMode_Config_CNF
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 2
- Message Structure:
CMAC_SecurityMode_Config_CNF
. (IntegerType)cellId = 0
- Constraint:
ca_CMAC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 00

- No.: 817
- Timestamp: 20:43:59:743_0
- RFN: 2415
- Chip: 14336
- Event: Send
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_REQ
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 3
- Message Structure:
CRLC_SecurityMode_Config_REQ
. (IntegerType)cellId = -1
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity = 1
. . (BitStringType)startValue[20] = "00000000000000000100"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = -
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CRLC_SecurityModeCfgReq
- BinaryMessage:
30 0e 02 01 ff 30 09 0a 01 01 03 04 04 00 00 40

- No.: 818
- Timestamp: 20:43:59:745_0
- RFN: 2415
- Chip: 21760
- Event: Receive
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_CNF
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 4
- Message Structure:
CRLC_SecurityMode_Config_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 832
- Timestamp: 20:43:59:750_0
- RFN: 2416
- Chip: 3328
- Event: Send
- PCO: CMAC
- Message: CMAC_SecurityMode_Config_REQ
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 1
- Message Structure:
CMAC_SecurityMode_Config_REQ
. (IntegerType)cellId = 0
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity = 0
. . (BitStringType)startValue[20] = "00000000000000000010"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = -
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CMAC_SecurityModeCfgReq
- BinaryMessage:
30 0e 02 01 00 30 09 0a 01 00 03 04 04 00 00 20

- No.: 833
- Timestamp: 20:43:59:752_0
- RFN: 2416
- Chip: 9728
- Event: Receive
- PCO: CMAC
- Message: CMAC_SecurityMode_Config_CNF
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 2
- Message Structure:
CMAC_SecurityMode_Config_CNF
. (IntegerType)cellId = 0
- Constraint:
ca_CMAC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 00

- No.: 834
- Timestamp: 20:43:59:754_0
- RFN: 2416
- Chip: 17408
- Event: Send
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_REQ
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 3
- Message Structure:
CRLC_SecurityMode_Config_REQ
. (IntegerType)cellId = -1
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity = 0
. . (BitStringType)startValue[20] = "00000000000000000010"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = -
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CRLC_SecurityModeCfgReq
- BinaryMessage:
30 0e 02 01 ff 30 09 0a 01 00 03 04 04 00 00 20

- No.: 835
- Timestamp: 20:43:59:756_0
- RFN: 2416
- Chip: 23808
- Event: Receive
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_CNF
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 4
- Message Structure:
CRLC_SecurityMode_Config_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 842
- Timestamp: 20:43:59:809_0
- RFN: 2421
- Chip: 36864
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_GMM_IdleUpdated:lt_IdleUpdated_NMO_II LINE 3
- Message Structure:
RRC_DataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain = 0
. (START_Value)start[20] = '00000000000000000010'B
. LOCATIONUPDATINGREQUEST
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)mMProtocolDiscriminator[4] = '0101'B
. . (MsgType)msgType[8] = '00001000'B
. . CiphKeySeqNum
. . . (B1)spare1[1] = '0'B
. . . (KeySeq)keySeq[3] = '000'B
. . LocUpdType
. . . (B1)fOR[1] = '0'B
. . . (B1)spare1[1] = '0'B
. . . (B2)lUT[2] = '10'B
. . LocAreaId_v
. . . (OctetStringType)plmn[3] = '00F110'O
. . . (OctetStringType)lac[2] = '0001'O
. . MS_Clsmk1
. . . (B1)spare1[1] = '0'B
. . . (B2)revLvl[2] = '10'B
. . . (B1)eSIND[1] = '0'B
. . . (B1)a5_1[1] = '1'B
. . . (B3)rFPwrCap[3] = '111'B
. . MS_Identity_lv
. . . (Length)iel[1] = '05'O
. . . (B4)iDigit1[4] = '1111'B
. . . (B1)oddEvenInd[1] = '0'B
. . . (B3)typeOfId[3] = '100'B
. . . (OctetStringType)otherDigits[4] = '12345678'O
. . MS_Clsmk2
. . . (IEI8)iei[8] = '00110011'B
. . . (Length)iel[1] = '03'O
. . . (B1)spare1_1[1] = '0'B
. . . (B2)revLvl[2] = '10'B
. . . (B1)eSIND[1] = '0'B
. . . (B1)a5_1[1] = '1'B
. . . (B3)rFPwrCap[3] = '111'B
. . . (B1)spare1_2[1] = '0'B
. . . (B1)pSCap[1] = '0'B
. . . (B2)sSSI[2] = '01'B
. . . (B1)sMCap[1] = '1'B
. . . (B1)vBS[1] = '0'B
. . . (B1)vGCS[1] = '0'B
. . . (B1)fC[1] = '0'B
. . . (B1)cM3[1] = '1'B
. . . (B1)spare1_3[1] = '0'B
. . . (B1)lCSVA[1] = '0'B
. . . (B1)uCS2[1] = '0'B
. . . (B1)soLSA[1] = '0'B
. . . (B1)cMSP[1] = '0'B
. . . (B1)a5_3[1] = '0'B
. . . (B1)a5_2[1] = '0'B
- Constraint:
car_InitDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 00 03 04 04 00 00 20 05 08 02 00 f1 10 00 01 4f 05 f4 12 34 56 78 33 03 4f 18 80

- No.: 879
- Timestamp: 20:43:59:869_0
- RFN: 2427
- Chip: 36096
- Event: Send
- PCO: Dc
- Message: RRC_DataReq
- Source: ts_MM_Authentication LINE 2
- Message Structure:
RRC_DataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[-1] = -
. (SapId)sapId[1] = -
. (SS_CN_DomainIdentity)cN_Domain = 0
. AUTHENTICATIONREQUEST
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)mMProtocolDiscriminator[4] = '0101'B
. . (MsgType)msgType[8] = '00010010'B
. . (B4)spare4[4] = '0000'B
. . CiphKeySeqNum
. . . (B1)spare1[1] = '0'B
. . . (KeySeq)keySeq[3] = '000'B
. . (MM_RAND)rAND[128] = '01010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101'B
. . AUTN
. . . (IEI8)iei[8] = '00100000'B
. . . (Length)iel[1] = '10'O
. . . (BitStringType)aUTN[128] = '01010110010100010101000001010011010100100101110100000000000000000101010101010100010101110101011001010001010100000101001101010010'B
- Constraint:
ca_DataReq
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 00 05 12 00 55 55 55 55 55 55 55 55 55 55 55 55 55 55 55 55 20 10 56 51 50 53 52 5d 00 00 55 54 57 56 51 50 53 52

- No.: 883
- Timestamp: 20:44:00:475_0
- RFN: 2488
- Chip: 19968
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_MM_Authentication LINE 7
- Message Structure:
RRC_DataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain = 0
. (START_Value)start[0] = -
. AUTHENTICATIONRESPONSE
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)mMProtocolDiscriminator[4] = '0101'B
. . (MsgType)msgType[8] = '01010100'B
. . (AuthRsp)authRsp[32] = '01010101010101000101011101010110'B
. . AuthRspExt
- Constraint:
car_UplinkDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 00 05 54 55 54 57 56

- No.: 921
- Timestamp: 20:44:00:510_0
- RFN: 2492
- Chip: 0
- Event: Send
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_REQ
- Source: ts_SS_DownloadSecurityKey:lt_DownloadKeyCRLC LINE 1
- Message Structure:
CRLC_SecurityMode_Config_REQ
. (IntegerType)cellId = -1
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity = 0
. . (BitStringType)startValue[20] = "00000000000000000000"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = '01010111010101100101000101010000010100110101001001011101010111000101111101011110010110010101100001011011010110100101010101010100'B
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CRLC_SecurityModeCfgReq
- BinaryMessage:
30 21 02 01 ff 30 1c 0a 01 00 03 04 04 00 00 00 03 11 00 57 56 51 50 53 52 5d 5c 5f 5e 59 58 5b 5a 55 54

- No.: 922
- Timestamp: 20:44:00:512_0
- RFN: 2492
- Chip: 6912
- Event: Receive
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_CNF
- Source: ts_SS_DownloadSecurityKey:lt_DownloadKeyCRLC LINE 2
- Message Structure:
CRLC_SecurityMode_Config_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 929
- Timestamp: 20:44:00:520_0
- RFN: 2493
- Chip: 1792
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 1
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
. (IntegerType)count_I_LSB_UL = -
. (IntegerType)count_I_LSB_DL = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 00 02 01 00 02 01 00

- No.: 930
- Timestamp: 20:44:00:522_0
- RFN: 2493
- Chip: 9984
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 2
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 00 02 01 00

- No.: 931
- Timestamp: 20:44:00:524_0
- RFN: 2493
- Chip: 17408
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 3
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. (IntegerType)count_I_LSB_UL = -
. (IntegerType)count_I_LSB_DL = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 01 02 01 00

- No.: 932
- Timestamp: 20:44:00:526_0
- RFN: 2493
- Chip: 24320
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 4
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 933
- Timestamp: 20:44:00:528_0
- RFN: 2493
- Chip: 31744
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 5
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. (IntegerType)count_I_LSB_UL = -
. (IntegerType)count_I_LSB_DL = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 02 02 01 00

- No.: 934
- Timestamp: 20:44:00:530_0
- RFN: 2494
- Chip: 768
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 6
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 935
- Timestamp: 20:44:00:532_0
- RFN: 2494
- Chip: 7936
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 7
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
. (IntegerType)count_I_LSB_UL = -
. (IntegerType)count_I_LSB_DL = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 03 02 01 00

- No.: 936
- Timestamp: 20:44:00:534_0
- RFN: 2494
- Chip: 15360
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 8
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 937
- Timestamp: 20:44:00:536_0
- RFN: 2494
- Chip: 22272
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 9
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
. (IntegerType)count_I_LSB_UL = -
. (IntegerType)count_I_LSB_DL = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 04 02 01 00

- No.: 938
- Timestamp: 20:44:00:537_0
- RFN: 2494
- Chip: 29440
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 10
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 942
- Timestamp: 20:44:00:550_0
- RFN: 2496
- Chip: 1536
- Event: Send
- PCO: CRLC
- Message: CRLC_Integrity_Activate_REQ
- Source: ts_CRLC_DL_Integrity LINE 1
- Message Structure:
CRLC_Integrity_Activate_REQ
. (IntegerType)cellId = -1
. (CN_DomainIdentity)cn_DomainIdentity = 0
. IntegrityActivationInfo
. . IntegrityProtectionModeInfo
. . . IntegrityProtectionModeCommand
. . . . startIntegrityProtection
. . . . . (BitStringType)integrityProtInitNumber[32] = "00000000000000000000000000000001"
. . . (IntegrityProtectionAlgorithm)integrityProtectionAlgorithm = 0
- Constraint:
ca_CRLC_DL_IntegrityActivateReq
- BinaryMessage:
30 15 02 01 ff 0a 01 00 30 0d 30 30 07 03 05 00 00 00 00 01 0a 01 00

- No.: 943
- Timestamp: 20:44:00:552_0
- RFN: 2496
- Chip: 8192
- Event: Receive
- PCO: CRLC
- Message: CRLC_Integrity_Activate_CNF
- Source: ts_CRLC_DL_Integrity LINE 2
- Message Structure:
CRLC_Integrity_Activate_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_IntegrityActivateCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 950
- Timestamp: 20:44:00:563_0
- RFN: 2497
- Chip: 12032
- Event: Send
- PCO: CRLC
- Message: CRLC_Integrity_Activate_REQ
- Source: ts_RB2_UL_IntegrityActivate LINE 1
- Message Structure:
CRLC_Integrity_Activate_REQ
. (IntegerType)cellId = -1
. (CN_DomainIdentity)cn_DomainIdentity = 0
. IntegrityActivationInfo
. . IntegrityProtActivationInfoList
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity = 2
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
- Constraint:
ca_CRLC_UL_IntegrityActivateReq
- BinaryMessage:
30 10 02 01 ff 0a 01 00 30 08 30 06 02 01 02 02 01 00

- No.: 951
- Timestamp: 20:44:00:565_0
- RFN: 2497
- Chip: 19200
- Event: Receive
- PCO: CRLC
- Message: CRLC_Integrity_Activate_CNF
- Source: ts_RB2_UL_IntegrityActivate LINE 2
- Message Structure:
CRLC_Integrity_Activate_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_IntegrityActivateCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 957
- Timestamp: 20:44:00:579_0
- RFN: 2498
- Chip: 34304
- Event: Send
- PCO: AM
- Message: RLC_AM_DATA_REQ
- Source: ts_RRC_Security:lt_SendSecurityModeCommand LINE 7
- Message Structure:
RLC_AM_DATA_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. AmConfirmationRequest
. aM_message
. . DL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00000000000000000000000000000000"
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . DL_DCCH_MessageType
. . . . SecurityModeCommand
. . . . . r3
. . . . . . SecurityModeCommand_r3_IEs
. . . . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . . . SecurityCapability
. . . . . . . . (BitStringType)cipheringAlgorithmCap[16] = '0000000000000011'B
. . . . . . . . (BitStringType)integrityProtectionAlgorithmCap[16] = '0000000000000010'B
. . . . . . . CipheringModeInfo
. . . . . . . IntegrityProtectionModeInfo
. . . . . . . . IntegrityProtectionModeCommand
. . . . . . . . . startIntegrityProtection
. . . . . . . . . . (BitStringType)integrityProtInitNumber[32] = "00000000000000000000000000000001"
. . . . . . . . (IntegrityProtectionAlgorithm)integrityProtectionAlgorithm = 0
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity = 0
. . . . . . . InterRAT_UE_SecurityCapList
. . . . . . laterNonCriticalExtensions
- Constraint:
cas_RRC_SecModeCmd
- BinaryMessage:
30 17 02 01 ff 02 01 02 05 00 80 00 00 00 04 04 00 01 80 01 40 00 00 00 20

- No.: 963
- Timestamp: 20:44:00:723_0
- RFN: 2513
- Chip: 13056
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_IND
- Source: ts_RRC_Security:lt_StartSecurity_UE LINE 8
- Message Structure:
RLC_AM_DATA_IND
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. IntegrityResult
. . (IntegrityStatus)integrityUsed = 0
. aM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "10000001100000001110110111011101"
. . . . (IntegerType)rrc_MessageSequenceNumber = 1
. . . UL_DCCH_MessageType
. . . . SecurityModeComplete
. . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . IntegrityProtActivationInfo
. . . . . . RRC_MessageSequenceNumberList
. . . . . . . (IntegerType)_elem = 0
. . . . . . . (IntegerType)_elem = 0
. . . . . . . (IntegerType)_elem = 0
. . . . . . . (IntegerType)_elem = 0
. . . . . . . (IntegerType)_elem = 0
. . . . . laterNonCriticalExtensions
. . . . . . (BitStringType)securityModeComplete_r3_add_ext = 0
. . . . . . nonCriticalExtensions
- Constraint:
car_RRC_SecModeCmpl
- BinaryMessage:
30 12 02 01 ff 02 01 02 0a 01 00 c0 c0 76 ee 8d 21 00 00 00

- No.: 964
- Timestamp: 20:44:00:724_0
- RFN: 2513
- Chip: 17408
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_Security:lt_StartSecurity_UE LINE 8
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 966
- Timestamp: 20:44:00:728_0
- RFN: 2513
- Chip: 32512
- Event: Send
- PCO: CRLC
- Message: CRLC_Integrity_Activate_REQ
- Source: ts_CRLC_UL_Integrity LINE 1
- Message Structure:
CRLC_Integrity_Activate_REQ
. (IntegerType)cellId = -1
. (CN_DomainIdentity)cn_DomainIdentity = 0
. IntegrityActivationInfo
. . IntegrityProtActivationInfoList
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity = 0
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity = 1
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity = 3
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity = 4
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
- Constraint:
ca_CRLC_UL_IntegrityActivateReq
- BinaryMessage:
30 28 02 01 ff 0a 01 00 30 20 30 06 02 01 00 02 01 00 30 06 02 01 01 02 01 00 30 06 02 01 03 02 01 00 30 06 02 01 04 02 01 00

- No.: 967
- Timestamp: 20:44:00:730_0
- RFN: 2514
- Chip: 1280
- Event: Receive
- PCO: CRLC
- Message: CRLC_Integrity_Activate_CNF
- Source: ts_CRLC_UL_Integrity LINE 2
- Message Structure:
CRLC_Integrity_Activate_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_IntegrityActivateCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 974
- Timestamp: 20:44:00:770_0
- RFN: 2518
- Chip: 1792
- Event: Send
- PCO: Dc
- Message: RRC_DataReq
- Source: ts_GMM_IdleUpdated:lt_LocUpdAcc LINE 2
- Message Structure:
RRC_DataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[-1] = -
. (SapId)sapId[1] = -
. (SS_CN_DomainIdentity)cN_Domain = 0
. LOCATIONUPDATINGACCEPT
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)mMProtocolDiscriminator[4] = '0101'B
. . (MsgType)msgType[8] = '00000010'B
. . LocAreaId_v
. . . (OctetStringType)plmn[3] = '00F110'O
. . . (OctetStringType)lac[2] = '0001'O
. . MM_MS_Identity
. . . (IEI8)iei[8] = '00010111'B
. . . (Length)iel[1] = '05'O
. . . (B4)iDigit1[4] = '1111'B
. . . (B1)oddEvenInd[1] = '0'B
. . . (B3)typeOfId[3] = '100'B
. . . (OctetStringType)otherDigits[-1] = '12345678'O
. . (FollowOnProceed)followOnProceed[8] = '10100001'B
. . (CTSPerm)cTSPerm[8] = '10100010'B
. . PLMN_List
- Constraint:
ca_DataReq
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 00 05 02 00 f1 10 00 01 17 05 f4 12 34 56 78 a1 a2

- No.: 978
- Timestamp: 20:44:00:929_0
- RFN: 2533
- Chip: 35072
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_GMM_IdleUpdated:lt_LocUpdAcc LINE 3
- Message Structure:
RRC_DataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain = 0
. (START_Value)start[0] = -
. TMSIREALLOCATIONCOMPLETE
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)mMProtocolDiscriminator[4] = '0101'B
. . (MsgType)msgType[8] = '10011011'B
- Constraint:
car_UplinkDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 00 05 9b

- No.: 992
- Timestamp: 20:44:00:945_1
- RFN: 2535
- Chip: 20992
- Event: Start Timer
- Source: ts_RRC_Delay LINE 1
- Message Structure:
no details available
- Constraint:
t_Dly (1000 Ms)
- BinaryMessage:

- No.: 996
- Timestamp: 20:44:01:938_0
- RFN: 2634
- Chip: 33536
- Event: Timeout
- Source: ts_RRC_Delay LINE 2
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 1001
- Timestamp: 20:44:01:949_0
- RFN: 2636
- Chip: 512
- Event: Send
- PCO: UM
- Message: RLC_UM_DATA_REQ
- Source: ts_RRC_ConnRel:lt_Send_RRC_ConnectionRelease LINE 3
- Message Structure:
RLC_UM_DATA_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. uM_message
. . DL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00000000000000000000000000000000"
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . DL_DCCH_MessageType
. . . . RRCConnectionRelease
. . . . . r3
. . . . . . RRCConnectionRelease_r3_IEs
. . . . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . . . (IntegerType)n_308 = 1
. . . . . . . (ReleaseCause)releaseCause = 0
. . . . . . . Rplmn_Information
. . . . . . laterNonCriticalExtensions
. (BooleanType)specialLI = FALSE
- Constraint:
cas_RRC_ConnRelDCCH
- BinaryMessage:
30 10 02 01 ff 02 01 01 80 00 00 00 03 c8 00 01 01 00

- No.: 1005
- Timestamp: 20:44:02:082_0
- RFN: 2649
- Chip: 9216
- Event: Receive
- PCO: UM
- Message: RLC_UM_DATA_IND
- Source: ts_RRC_ConnRel:lt_Send_RRC_ConnectionRelease LINE 4
- Message Structure:
RLC_UM_DATA_IND
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. IntegrityResult
. uM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "10101101101011101001000000111001"
. . . . (IntegerType)rrc_MessageSequenceNumber = 1
. . . UL_DCCH_MessageType
. . . . RRCConnectionReleaseComplete
. . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . FailureCauseWithProtErr
. . . . . laterNonCriticalExtensions
. . . . . . (BitStringType)rrcConnectionReleaseComplete_r3_add_ext = 0
. . . . . . nonCriticalExtensions
- Constraint:
car_RRC_ConnRelCmplUM
- BinaryMessage:
30 0c 02 01 ff 02 01 01 d6 d7 48 1c 8c 40

- No.: 1006
- Timestamp: 20:44:02:083_0
- RFN: 2649
- Chip: 12800
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ConnRel:lt_Send_RRC_ConnectionRelease LINE 4
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1009
- Timestamp: 20:44:02:085_0
- RFN: 2649
- Chip: 17664
- Event: Start Timer
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 1
- Message Structure:
no details available
- Constraint:
t_Dly (5000 Ms)
- BinaryMessage:

- No.: 1013
- Timestamp: 20:44:02:231_0
- RFN: 2664
- Chip: 7168
- Event: Receive
- PCO: UM
- Message: RLC_UM_DATA_IND
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 4
- Message Structure:
RLC_UM_DATA_IND
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. IntegrityResult
. uM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00011100010101000111110101101001"
. . . . (IntegerType)rrc_MessageSequenceNumber = 2
. . . UL_DCCH_MessageType
. . . . RRCConnectionReleaseComplete
. . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . FailureCauseWithProtErr
. . . . . laterNonCriticalExtensions
. . . . . . (BitStringType)rrcConnectionReleaseComplete_r3_add_ext = 0
. . . . . . nonCriticalExtensions
- Constraint:
car_RRC_ConnRelCmplUM
- BinaryMessage:
30 0c 02 01 ff 02 01 01 8e 2a 3e b4 94 40

- No.: 1014
- Timestamp: 20:44:02:232_0
- RFN: 2664
- Chip: 11264
- Event: Cancel Timer
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 4
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 1015
- Timestamp: 20:44:02:233_0
- RFN: 2664
- Chip: 12032
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 4
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1021
- Timestamp: 20:44:02:236_0
- RFN: 2664
- Chip: 26624
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 01 0a 01 00 05 00

- No.: 1025
- Timestamp: 20:44:02:243_0
- RFN: 2665
- Chip: 12544
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 1028
- Timestamp: 20:44:02:246_0
- RFN: 2665
- Chip: 24064
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 02 0a 01 00 05 00

- No.: 1032
- Timestamp: 20:44:02:253_0
- RFN: 2666
- Chip: 13824
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 1035
- Timestamp: 20:44:02:256_0
- RFN: 2666
- Chip: 24320
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 03 0a 01 00 05 00

- No.: 1039
- Timestamp: 20:44:02:268_0
- RFN: 2667
- Chip: 34304
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 1042
- Timestamp: 20:44:02:271_0
- RFN: 2668
- Chip: 7680
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 04 0a 01 00 05 00

- No.: 1046
- Timestamp: 20:44:02:280_0
- RFN: 2669
- Chip: 4864
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 1049
- Timestamp: 20:44:02:288_0
- RFN: 2669
- Chip: 33792
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 136
. . . . . UL_RLC_Mode
. . . . . . UL_UM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (NoExplicitDiscard)timerBasedNoExplicit = 9
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = 1
. . . . (IntegerType)dLlogicalChannelIdentity = 1
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_UM_Info
- BinaryMessage:
30 22 02 01 ff 02 01 01 0a 01 00 30 17 30 0d 05 00 30 09 02 02 00 88 30 03 0a 01 09 30 06 02 01 01 02 01 01

- No.: 1053
- Timestamp: 20:44:02:298_0
- RFN: 2670
- Chip: 32512
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 1054
- Timestamp: 20:44:02:306_0
- RFN: 2671
- Chip: 27136
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 3
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . (TimerEPC)timerEPC = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . (TimerRST)timerRST = 9
. . . . . . . (MaxRST)max_RST = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = 2
. . . . (IntegerType)dLlogicalChannelIdentity = 2
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 02 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 27 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 02 02 01 02

- No.: 1058
- Timestamp: 20:44:02:328_0
- RFN: 2673
- Chip: 33792
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 4
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 1059
- Timestamp: 20:44:02:336_0
- RFN: 2674
- Chip: 27648
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 5
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . (TimerEPC)timerEPC = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . (TimerRST)timerRST = 9
. . . . . . . (MaxRST)max_RST = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = 3
. . . . (IntegerType)dLlogicalChannelIdentity = 3
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 03 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 27 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 03 02 01 03

- No.: 1063
- Timestamp: 20:44:02:361_0
- RFN: 2677
- Chip: 2048
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 6
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 1064
- Timestamp: 20:44:02:375_0
- RFN: 2678
- Chip: 21248
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 7
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . (TimerEPC)timerEPC = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . (TimerRST)timerRST = 9
. . . . . . . (MaxRST)max_RST = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = 4
. . . . (IntegerType)dLlogicalChannelIdentity = 4
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 04 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 27 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 04 02 01 04

- No.: 1068
- Timestamp: 20:44:02:399_0
- RFN: 2680
- Chip: 34816
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 8
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 1091
- Timestamp: 20:44:02:407_0
- RFN: 2681
- Chip: 26112
- Event: Start Timer
- Source: ts_GMM_IdleUpdated:lt_HandleAttachRequest LINE 5
- Message Structure:
no details available
- Constraint:
t_WaitS (1 Sec)
- BinaryMessage:

- No.: 1095
- Timestamp: 20:44:03:402_0
- RFN: 2781
- Chip: 9216
- Event: Timeout
- Source: ts_GMM_IdleUpdated:lt_HandleAttachRequest LINE 6
- Message Structure:
no details available
- Constraint:
t_WaitS
- BinaryMessage:

- No.: 1097
- Timestamp: 20:44:03:403_1
- RFN: 2781
- Chip: 12800
- Event: Start Timer
- Source: ts_GMM_IdleUpdated:lt_HandleAttachRequest LINE 7
- Message Structure:
no details available
- Constraint:
t_WaitS (60 Sec)
- BinaryMessage:

- No.: 1099
- Timestamp: 20:44:03:405_0
- RFN: 2781
- Chip: 21504
- Event: Send
- PCO: Ut
- Message: AT_CmdReq
- Source: ts_AT_TriggerGMM_Attach LINE 1
- Message Structure:
AT_CmdReq
. (IA5StringType)cmd[-1] = "AT+CGATT=1"
. (HexStringType)sMS_BlockMode[-1] = -
- Constraint:
ca_AT_CmdReq
- BinaryMessage:
41 54 2b 43 47 41 54 54 3d 31 3c 43 52 3e

- No.: 1103
- Timestamp: 20:44:04:532_0
- RFN: 2894
- Chip: 10752
- Event: Receive
- PCO: Ut
- Message: AT_CmdCnf
- Source: ts_AT_TriggerGMM_Attach LINE 2
- Message Structure:
AT_CmdCnf
. (BooleanType)result = TRUE
. (IA5StringType)resultString[18] = "OK"
. (HexStringType)sMS_BlockMode[0] = -
- Constraint:
ca_AT_CmdCnf
- BinaryMessage:
80 3c 43 52 3e 3c 4c 46 3e 4f 4b 3c 43 52 3e 3c 4c 46 3e

- No.: 1120
- Timestamp: 20:44:04:540_0
- RFN: 2894
- Chip: 37120
- Event: Receive
- PCO: CPHY
- Message: CPHY_Out_of_Sync_IND
- Source: RRC_DefConnEst LINE 7
- Message Structure:
CPHY_Out_of_Sync_IND
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_OutOfSyncInd
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 1121
- Timestamp: 20:44:04:540_1
- RFN: 2895
- Chip: 768
- Event: Cancel Timer
- Source: RRC_DefConnEst LINE 7
- Message Structure:
no details available
- Constraint:
t_T312
- BinaryMessage:

- No.: 1122
- Timestamp: 20:44:04:541_0
- RFN: 2895
- Chip: 2560
- Event: Default
- Source: RRC_DefConnEst LINE 0
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1123
- Timestamp: 20:44:04:541_1
- RFN: 2895
- Chip: 3328
- Event: Default
- Source: ts_RRC_ConnEst:lt_RcvConnReq LINE 2
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1128
- Timestamp: 20:44:06:073_0
- RFN: 3048
- Chip: 15360
- Event: Receive
- PCO: TM
- Message: RLC_TR_DATA_IND
- Source: ts_RRC_ConnEst:lt_RcvConnReq LINE 2
- Message Structure:
RLC_TR_DATA_IND
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
. tM_message
. . UL_CCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode = 0
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . UL_CCCH_MessageType
. . . . RRCConnectionRequest
. . . . . InitialUE_Identity
. . . . . . TMSI_and_LAI_GSM_MAP
. . . . . . . (BitStringType)tmsi[32] = "00010010001101000101011001111000"
. . . . . . . LAI
. . . . . . . . PLMN_Identity
. . . . . . . . . MCC
. . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . (IntegerType)_elem = 1
. . . . . . . . . MNC
. . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . (IntegerType)_elem = 1
. . . . . . . . (BitStringType)lac[16] = '0000000000000001'B
. . . . . (EstablishmentCause)establishmentCause = 12
. . . . . (ProtocolErrorIndicator)protocolErrorIndicator = 0
. . . . . MeasuredResultsOnRACH
. . . . . . currentCell
. . . . . . . modeSpecificInfo
. . . . . . . . fdd
. . . . . . . . . measurementQuantity
. . . . . . . . . . (IntegerType)cpich_Ec_N0 = 0
. . . . . v3d0NonCriticalExtensions
. . . . . . RRCConnectionRequest_v3d0ext_IEs
. . . . . . . (BitStringType)uESpecificBehaviourInformation1idle = 0
. . . . . . nonCriticalExtensions
- Constraint:
car_RRC_ConnReq
- BinaryMessage:
30 11 02 01 00 02 01 00 21 12 34 56 78 00 10 08 00 0b 00

- No.: 1132
- Timestamp: 20:44:06:135_0
- RFN: 3054
- Chip: 19712
- Event: Send
- PCO: UM
- Message: RLC_UM_DATA_REQ
- Source: ts_RRC_ConnEst:lt_Send_ConnSetUp LINE 22
- Message Structure:
RLC_UM_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
. uM_message
. . DL_CCCH_Message
. . . IntegrityCheckInfo
. . . DL_CCCH_MessageType
. . . . RRCConnectionSetup
. . . . . r3
. . . . . . RRCConnectionSetup_r3_IEs
. . . . . . . InitialUE_Identity
. . . . . . . . TMSI_and_LAI_GSM_MAP
. . . . . . . . . (BitStringType)tmsi[32] = "00010010001101000101011001111000"
. . . . . . . . . LAI
. . . . . . . . . . PLMN_Identity
. . . . . . . . . . . MCC
. . . . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . . . (IntegerType)_elem = 1
. . . . . . . . . . . MNC
. . . . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . . . (IntegerType)_elem = 1
. . . . . . . . . . (BitStringType)lac[16] = '0000000000000001'B
. . . . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . . . (IntegerType)activationTime = -
. . . . . . . U_RNTI
. . . . . . . . (BitStringType)srnc_Identity[12] = "000000000001"
. . . . . . . . (BitStringType)s_RNTI[20] = "00000000000000000001"
. . . . . . . (BitStringType)new_c_RNTI[16] = -
. . . . . . . (RRC_StateIndicator)rrc_StateIndicator = 0
. . . . . . . (IntegerType)utran_DRX_CycleLengthCoeff = 9
. . . . . . . CapabilityUpdateRequirement
. . . . . . . . (BooleanType)ue_RadioCapabilityFDDUpdateRequirement = TRUE
. . . . . . . . (BooleanType)ue_RadioCapabilityTDDUpdateRequirement = FALSE
. . . . . . . . SystemSpecificCapUpdateReqList
. . . . . . . . . (SystemSpecificCapUpdateReq)_elem = 0
. . . . . . . SRB_InformationSetupList2
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_UM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 1
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 1
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . . . . . . . (TimerRST)timerRST = 9
. . . . . . . . . . . . . (MaxRST)max_RST = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 2
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 2
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . . . . . . . (TimerRST)timerRST = 9
. . . . . . . . . . . . . (MaxRST)max_RST = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 3
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 3
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . . . . . . . (TimerRST)timerRST = 9
. . . . . . . . . . . . . (MaxRST)max_RST = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 4
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 4
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . UL_CommonTransChInfo
. . . . . . . . TFC_Subset
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . TFCS
. . . . . . . . . . . ExplicitTFCS_Configuration
. . . . . . . . . . . . TFCS_ReconfAdd
. . . . . . . . . . . . . ctfcSize
. . . . . . . . . . . . . . ctfc2Bit
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . . . . . . . (IntegerType)ctfc2 = 0
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . . . . . . . (IntegerType)ctfc2 = 1
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 11
. . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . UL_AddReconfTransChInfoList
. . . . . . . . UL_AddReconfTransChInformation
. . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType = 0
. . . . . . . . . (IntegerType)transportChannelIdentity = 5
. . . . . . . . . TransportFormatSet
. . . . . . . . . . DedicatedTransChTFS
. . . . . . . . . . . tti
. . . . . . . . . . . . DedicatedDynamicTF_InfoList
. . . . . . . . . . . . . DedicatedDynamicTF_Info
. . . . . . . . . . . . . . rlc_Size
. . . . . . . . . . . . . . . BitModeRLC_SizeInfo
. . . . . . . . . . . . . . . . sizeType2
. . . . . . . . . . . . . . . . . (IntegerType)part1 = 2
. . . . . . . . . . . . . . . . . (IntegerType)part2 = -
. . . . . . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . LogicalChannelList
. . . . . . . . . . . SemistaticTF_Information
. . . . . . . . . . . . ChannelCodingType
. . . . . . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . . . . . (IntegerType)rateMatchingAttribute = 192
. . . . . . . . . . . . (CRC_Size)crc_Size = 3
. . . . . . . DL_CommonTransChInfo
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . dl_Parameters
. . . . . . . DL_AddReconfTransChInfoList
. . . . . . . . DL_AddReconfTransChInformation
. . . . . . . . . (DL_TrCH_Type)dl_TransportChannelType = 0
. . . . . . . . . (IntegerType)dl_transportChannelIdentity = 10
. . . . . . . . . tfs_SignallingMode
. . . . . . . . . . UL_TransportChannelIdentity
. . . . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType = 0
. . . . . . . . . . . (IntegerType)ul_TransportChannelIdentity = 5
. . . . . . . . . QualityTarget
. . . . . . . . . . (IntegerType)bler_QualityValue = -20
. . . . . . . . . TM_SignallingInfo
. . . . . . . FrequencyInfo
. . . . . . . (IntegerType)maxAllowedUL_TX_Power = -
. . . . . . . UL_ChannelRequirement
. . . . . . . . UL_DPCH_Info
. . . . . . . . . UL_DPCH_PowerControlInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (IntegerType)dpcch_PowerOffset = -40
. . . . . . . . . . . (IntegerType)pc_Preamble = 1
. . . . . . . . . . . (IntegerType)sRB_delay = 7
. . . . . . . . . . . PowerControlAlgorithm
. . . . . . . . . . . . (IntegerType)algorithm1 = 1
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (ScramblingCodeType)scramblingCodeType = 1
. . . . . . . . . . . (IntegerType)scramblingCode = 0
. . . . . . . . . . . (IntegerType)numberOfDPDCH = -
. . . . . . . . . . . (SpreadingFactor)spreadingFactor = 4
. . . . . . . . . . . (BooleanType)tfci_Existence = TRUE
. . . . . . . . . . . (IntegerType)numberOfFBI_Bits = -
. . . . . . . . . . . (PuncturingLimit)puncturingLimit = 15
. . . . . . . DL_CommonInformation
. . . . . . . . DL_DPCH_InfoCommon
. . . . . . . . . cfnHandling
. . . . . . . . . . initialise
. . . . . . . . . . . (IntegerType)cfntargetsfnframeoffset = -
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . DL_DPCH_PowerControlInfo
. . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . (DPC_Mode)dpc_Mode = 0
. . . . . . . . . . . (IntegerType)powerOffsetPilot_pdpdch = 0
. . . . . . . . . . . Dl_rate_matching_restriction
. . . . . . . . . . . SF512_AndPilot
. . . . . . . . . . . . (PilotBits128)sfd128 = 0
. . . . . . . . . . . (PositionFixedOrFlexible)positionFixedOrFlexible = 0
. . . . . . . . . . . (BooleanType)tfci_Existence = FALSE
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . (IntegerType)defaultDPCH_OffsetValue = 0
. . . . . . . . . . DPCH_CompressedModeInfo
. . . . . . . . . . (TX_DiversityMode)tx_DiversityMode = 0
. . . . . . . . . . SSDT_Information
. . . . . . . DL_InformationPerRL_List
. . . . . . . . DL_InformationPerRL
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . PrimaryCPICH_Info
. . . . . . . . . . . . (IntegerType)primaryScramblingCode = 100
. . . . . . . . . . . PDSCH_SHO_DCH_Info
. . . . . . . . . . . PDSCH_CodeMapping
. . . . . . . . . DL_DPCH_InfoPerRL
. . . . . . . . . . fdd
. . . . . . . . . . . (PCPICH_UsageForChannelEst)pCPICH_UsageForChannelEst = 0
. . . . . . . . . . . (IntegerType)dpch_FrameOffset = 0
. . . . . . . . . . . SecondaryCPICH_Info
. . . . . . . . . . . DL_ChannelisationCodeList
. . . . . . . . . . . . DL_ChannelisationCode
. . . . . . . . . . . . . (IntegerType)secondaryScramblingCode = 1
. . . . . . . . . . . . . SF512_AndCodeNumber
. . . . . . . . . . . . . . (IntegerType)sf128 = 0
. . . . . . . . . . . . . (ScramblingCodeChange)scramblingCodeChange = 1
. . . . . . . . . . . (IntegerType)tpc_CombinationIndex = 0
. . . . . . . . . . . (SSDT_CellIdentity)ssdt_CellIdentity = -
. . . . . . . . . . . (ClosedLoopTimingAdjMode)closedLoopTimingAdjMode = -
. . . . . . . . . SCCPCH_InfoForFACH
. . . . . . laterNonCriticalExtensions
. (BooleanType)specialLI = TRUE
- Constraint:
cas_RRC_ConnSetup
- BinaryMessage:
30 78 02 01 00 02 01 00 30 e7 22 46 8a cf 00 02 01 00 01 00 04 00 00 4d 82 69 3a 10 10 89 0d 42 00 02 81 9e 8e 46 c9 ce 7c 9c 4e 74 20 a5 12 3a 8c 00 15 13 3d 1c 8d 93 9c f9 38 9c e8 42 52 24 b5 28 00 4a 46 7a 39 1b 27 39 f2 71 39 d0 86 b4 49 ea 70 00 d4 c8 00 06 25 2b f0 02 00 08 82 23 bf 66 08 98 95 a5 47 a2 00 00 01 3f 90 0a 14 00 02 06 40 00 0c 28 08 01 01 ff

- No.: 1153
- Timestamp: 20:44:06:178_2
- RFN: 3058
- Chip: 32768
- Event: Start Timer
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 3
- Message Structure:
no details available
- Constraint:
t_WaitMS (13500 Ms)
- BinaryMessage:

- No.: 1158
- Timestamp: 20:44:06:407_0
- RFN: 3081
- Chip: 30720
- Event: Receive
- PCO: CPHY
- Message: CPHY_Sync_IND
- Source: RRC_Def1 LINE 13
- Message Structure:
CPHY_Sync_IND
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_SyncInd
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 1159
- Timestamp: 20:44:06:408_0
- RFN: 3081
- Chip: 32512
- Event: Cancel Timer
- Source: RRC_Def1 LINE 13
- Message Structure:
no details available
- Constraint:
t_T312
- BinaryMessage:

- No.: 1160
- Timestamp: 20:44:06:408_1
- RFN: 3081
- Chip: 34816
- Event: Default
- Source: RRC_Def1 LINE 0
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1161
- Timestamp: 20:44:06:408_2
- RFN: 3081
- Chip: 35584
- Event: Default
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1166
- Timestamp: 20:44:06:523_0
- RFN: 3093
- Chip: 12032
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_IND
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
RLC_AM_DATA_IND
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. IntegrityResult
. . (IntegrityStatus)integrityUsed = 0
. aM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode = 0
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . UL_DCCH_MessageType
. . . . RRCConnectionSetupComplete
. . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . STARTList
. . . . . . STARTSingle
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity = 1
. . . . . . . (BitStringType)start_Value[20] = "00000000000000000100"
. . . . . . STARTSingle
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity = 0
. . . . . . . (BitStringType)start_Value[20] = "00000000000000000010"
. . . . . UE_RadioAccessCapability
. . . . . . (AccessStratumReleaseIndicator)accessStratumReleaseIndicator = 0
. . . . . . PDCP_Capability
. . . . . . . (BooleanType)losslessSRNS_RelocationSupport = FALSE
. . . . . . . supportForRfc2507
. . . . . . RLC_Capability
. . . . . . . (TotalRLC_AM_BufferSize)totalRLC_AM_BufferSize = 2
. . . . . . . (MaximumRLC_WindowSize)maximumRLC_WindowSize = 0
. . . . . . . (MaximumAM_EntityNumberRLC_Cap)maximumAM_EntityNumber = 3
. . . . . . TransportChannelCapability
. . . . . . . DL_TransChCapability
. . . . . . . . (MaxNoBits)maxNoBitsReceived = 4
. . . . . . . . (MaxNoBits)maxConvCodeBitsReceived = 1
. . . . . . . . TurboSupport
. . . . . . . . . (MaxNoBits)supported = 4
. . . . . . . . (MaxSimultaneousTransChsDL)maxSimultaneousTransChs = 1
. . . . . . . . (IntegerType)maxSimultaneousCCTrCH_Count = 1
. . . . . . . . (MaxTransportBlocksDL)maxReceivedTransportBlocks = 2
. . . . . . . . (MaxNumberOfTFC_DL)maxNumberOfTFC = 4
. . . . . . . . (MaxNumberOfTF)maxNumberOfTF = 1
. . . . . . . UL_TransChCapability
. . . . . . . . (MaxNoBits)maxNoBitsTransmitted = 3
. . . . . . . . (MaxNoBits)maxConvCodeBitsTransmitted = 1
. . . . . . . . TurboSupport
. . . . . . . . . (MaxNoBits)supported = 3
. . . . . . . . (MaxSimultaneousTransChsUL)maxSimultaneousTransChs = 2
. . . . . . . . modeSpecificInfo
. . . . . . . . (MaxTransportBlocksUL)maxTransmittedBlocks = 2
. . . . . . . . (MaxNumberOfTFC_UL)maxNumberOfTFC = 3
. . . . . . . . (MaxNumberOfTF)maxNumberOfTF = 0
. . . . . . RF_Capability
. . . . . . . fddRF_Capability
. . . . . . . . (IntegerType)ue_PowerClass = 4
. . . . . . . . (TxRxFrequencySeparation)txRxFrequencySeparation = 0
. . . . . . . tddRF_Capability
. . . . . . . . (IntegerType)ue_PowerClass = 0
. . . . . . . . (RadioFrequencyBandTDDList)radioFrequencyTDDBandList = 0
. . . . . . . . (ChipRateCapability)chipRateCapability = 0
. . . . . . PhysicalChannelCapability
. . . . . . . fddPhysChCapability
. . . . . . . . DL_PhysChCapabilityFDD
. . . . . . . . . (IntegerType)maxNoDPCH_PDSCH_Codes = 3
. . . . . . . . . (MaxNoPhysChBitsReceived)maxNoPhysChBitsReceived = 6
. . . . . . . . . (BooleanType)supportForSF_512 = FALSE
. . . . . . . . . (BooleanType)supportOfPDSCH = FALSE
. . . . . . . . . SimultaneousSCCPCH_DPCH_Reception
. . . . . . . . UL_PhysChCapabilityFDD
. . . . . . . . . (MaxNoDPDCH_BitsTransmitted)maxNoDPDCH_BitsTransmitted = 2
. . . . . . . . . (BooleanType)supportOfPCPCH = FALSE
. . . . . . . tddPhysChCapability
. . . . . . . . DL_PhysChCapabilityTDD
. . . . . . . . . (IntegerType)maxTS_PerFrame = 0
. . . . . . . . . (IntegerType)maxPhysChPerFrame = 0
. . . . . . . . . (MinimumSF_DL)minimumSF = 0
. . . . . . . . . (BooleanType)supportOfPDSCH = FALSE
. . . . . . . . . (IntegerType)maxPhysChPerTS = 0
. . . . . . . . UL_PhysChCapabilityTDD
. . . . . . . . . (IntegerType)maxTS_PerFrame = 0
. . . . . . . . . (MaxPhysChPerTimeslot)maxPhysChPerTimeslot = 0
. . . . . . . . . (MinimumSF_UL)minimumSF = 0
. . . . . . . . . (BooleanType)supportOfPUSCH = FALSE
. . . . . . UE_MultiModeRAT_Capability
. . . . . . . MultiRAT_Capability
. . . . . . . . (BooleanType)supportOfGSM = TRUE
. . . . . . . . (BooleanType)supportOfMulticarrier = FALSE
. . . . . . . (MultiModeCapability)multiModeCapability = 1
. . . . . . SecurityCapability
. . . . . . . (BitStringType)cipheringAlgorithmCap[16] = '0000000000000011'B
. . . . . . . (BitStringType)integrityProtectionAlgorithmCap[16] = '0000000000000010'B
. . . . . . UE_Positioning_Capability
. . . . . . . (BooleanType)standaloneLocMethodsSupported = FALSE
. . . . . . . (BooleanType)ue_BasedOTDOA_Supported = FALSE
. . . . . . . (NetworkAssistedGPS_Supported)networkAssistedGPS_Supported = 3
. . . . . . . (BooleanType)supportForUE_GPS_TimingOfCellFrames = FALSE
. . . . . . . (BooleanType)supportForIPDL = FALSE
. . . . . . MeasurementCapability
. . . . . . . CompressedModeMeasCapability
. . . . . . . . (BooleanType)fdd_Measurements = TRUE
. . . . . . . . (BooleanType)tdd_Measurements = FALSE
. . . . . . . . GSM_Measurements
. . . . . . . . . (BooleanType)gsm900 = TRUE
. . . . . . . . . (BooleanType)dcs1800 = TRUE
. . . . . . . . . (BooleanType)gsm1900 = FALSE
. . . . . . . . (BooleanType)multiCarrierMeasurements = FALSE
. . . . . . . CompressedModeMeasCapability
. . . . . . . . (BooleanType)fdd_Measurements = TRUE
. . . . . . . . (BooleanType)tdd_Measurements = FALSE
. . . . . . . . GSM_Measurements
. . . . . . . . . (BooleanType)gsm900 = TRUE
. . . . . . . . . (BooleanType)dcs1800 = TRUE
. . . . . . . . . (BooleanType)gsm1900 = FALSE
. . . . . . . . (BooleanType)multiCarrierMeasurements = FALSE
. . . . . v370NonCriticalExtensions
. . . . . . RRCConnectionSetupComplete_v370ext
. . . . . . . UE_RadioAccessCapability_v370ext
. . . . . . v380NonCriticalExtensions
. . . . . . . RRCConnectionSetupComplete_v380ext_IEs
. . . . . . . . UE_RadioAccessCapability_v380ext
. . . . . . . . . UE_PositioningCapabilityExt_v380
. . . . . . . . . . (BooleanType)rx_tx_TimeDifferenceType2Capable = FALSE
. . . . . . . . DL_PhysChCapabilityFDD_v380ext
. . . . . . . . . (SupportOfDedicatedPilotsForChEstimation)supportOfDedicatedPilotsForChEstimation = 0
. . . . . . . v3a0NonCriticalExtensions
. . . . . . . . RRCConnectionSetupComplete_v3a0ext_IEs
. . . . . . . . . UE_RadioAccessCapability_v3a0ext
. . . . . . . . . . UE_PositioningCapabilityExt_v3a0
. . . . . . . . . . . (UE_PositioningCapabilityExt_v3a0_list_0)validity_CellPCH_UraPCH = 0
. . . . . . . . laterNonCriticalExtensions
. . . . . . . . . (BitStringType)rrcConnectionSetupComplete_r3_add_ext = 0
. . . . . . . . . nonCriticalExtensions
- Constraint:
car_RRC_ConnSetupCmpl
- BinaryMessage:
30 27 02 01 ff 02 01 02 0a 05 01 00 00 00 00 4a 0c 00 01 00 00 05 11 a0 d1 04 84 c6 68 46 2c 93 02 48 00 18 00 11 8f 8f 80

- No.: 1167
- Timestamp: 20:44:06:531_0
- RFN: 3094
- Chip: 3328
- Event: Cancel Timer
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
t_WaitMS
- BinaryMessage:

- No.: 1168
- Timestamp: 20:44:06:531_1
- RFN: 3094
- Chip: 4096
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1182
- Timestamp: 20:44:06:539_0
- RFN: 3094
- Chip: 37120
- Event: Send
- PCO: CMAC
- Message: CMAC_SecurityMode_Config_REQ
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 1
- Message Structure:
CMAC_SecurityMode_Config_REQ
. (IntegerType)cellId = 0
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity = 1
. . (BitStringType)startValue[20] = "00000000000000000100"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = -
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CMAC_SecurityModeCfgReq
- BinaryMessage:
30 0e 02 01 00 30 09 0a 01 01 03 04 04 00 00 40

- No.: 1183
- Timestamp: 20:44:06:542_0
- RFN: 3095
- Chip: 7424
- Event: Receive
- PCO: CMAC
- Message: CMAC_SecurityMode_Config_CNF
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 2
- Message Structure:
CMAC_SecurityMode_Config_CNF
. (IntegerType)cellId = 0
- Constraint:
ca_CMAC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 00

- No.: 1184
- Timestamp: 20:44:06:543_0
- RFN: 3095
- Chip: 14336
- Event: Send
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_REQ
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 3
- Message Structure:
CRLC_SecurityMode_Config_REQ
. (IntegerType)cellId = -1
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity = 1
. . (BitStringType)startValue[20] = "00000000000000000100"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = -
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CRLC_SecurityModeCfgReq
- BinaryMessage:
30 0e 02 01 ff 30 09 0a 01 01 03 04 04 00 00 40

- No.: 1185
- Timestamp: 20:44:06:545_0
- RFN: 3095
- Chip: 20480
- Event: Receive
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_CNF
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 4
- Message Structure:
CRLC_SecurityMode_Config_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1199
- Timestamp: 20:44:06:550_0
- RFN: 3096
- Chip: 1280
- Event: Send
- PCO: CMAC
- Message: CMAC_SecurityMode_Config_REQ
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 1
- Message Structure:
CMAC_SecurityMode_Config_REQ
. (IntegerType)cellId = 0
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity = 0
. . (BitStringType)startValue[20] = "00000000000000000010"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = -
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CMAC_SecurityModeCfgReq
- BinaryMessage:
30 0e 02 01 00 30 09 0a 01 00 03 04 04 00 00 20

- No.: 1200
- Timestamp: 20:44:06:552_0
- RFN: 3096
- Chip: 7680
- Event: Receive
- PCO: CMAC
- Message: CMAC_SecurityMode_Config_CNF
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 2
- Message Structure:
CMAC_SecurityMode_Config_CNF
. (IntegerType)cellId = 0
- Constraint:
ca_CMAC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 00

- No.: 1201
- Timestamp: 20:44:06:553_0
- RFN: 3096
- Chip: 14592
- Event: Send
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_REQ
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 3
- Message Structure:
CRLC_SecurityMode_Config_REQ
. (IntegerType)cellId = -1
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity = 0
. . (BitStringType)startValue[20] = "00000000000000000010"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = -
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CRLC_SecurityModeCfgReq
- BinaryMessage:
30 0e 02 01 ff 30 09 0a 01 00 03 04 04 00 00 20

- No.: 1202
- Timestamp: 20:44:06:555_0
- RFN: 3096
- Chip: 20480
- Event: Receive
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_CNF
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 4
- Message Structure:
CRLC_SecurityMode_Config_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1209
- Timestamp: 20:44:06:586_0
- RFN: 3099
- Chip: 24832
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_GMM_IdleUpdated:lt_HandleAttachRequest LINE 10
- Message Structure:
RRC_DataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. (START_Value)start[20] = '00000000000000000100'B
. ATTACHREQUEST
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)gMMProtocolDiscriminator[4] = '1000'B
. . (MsgType)msgType[8] = '00000001'B
. . MS_NetworkCap_lv
. . . (Length)iel[1] = '02'O
. . . (OctetStringType)value[2] = 'E540'O
. . CiphKeySeqNum
. . . (B1)spare1[1] = '0'B
. . . (KeySeq)keySeq[3] = '000'B
. . AttachType
. . . (B1)pre_for[1] = '0'B
. . . (B3)type[3] = '001'B
. . DRXparamter
. . . (B8)splitPGcycleCode[8] = '00000111'B
. . . (B4)cnDRXcoef[4] = '0000'B
. . . (B1)splitOnCCCH[1] = '0'B
. . . (B3)nonDRXtimer[3] = '010'B
. . MS_Identity_lv
. . . (Length)iel[1] = '05'O
. . . (B4)iDigit1[4] = '1111'B
. . . (B1)oddEvenInd[1] = '0'B
. . . (B3)typeOfId[3] = '100'B
. . . (OctetStringType)otherDigits[4] = '12345678'O
. . RAI_v
. . . (OctetStringType)plmn[3] = '00F110'O
. . . (OctetStringType)lac[2] = '0001'O
. . . (OctetStringType)rac[1] = '05'O
. . MSRadioAccessCap_lv
. . . (Length)iel[1] = '0A'O
. . . (OctetStringType)value[10] = '14F382334C03263CA060'O
. . PTMSI_Signature
. . . (IEI8)iei[8] = '00010111'B
. . . (OctetStringType)value[3] = -
. . GPRS_Timer
. . . (IEI8)iei[8] = '00010110'B
. . . (B3)unit[0] = -
. . . (B5)value[0] = -
. . TMSI_Status
. . . (IEI4)iei[0] = -
. . . (B3)spare3[0] = -
. . . (B1)flag[0] = -
- Constraint:
car_PS_InitDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 03 04 04 00 00 40 08 01 02 e5 40 01 07 02 05 f4 12 34 56 78 00 f1 10 00 01 05 0a 14 f3 82 33 4c 03 26 3c a0 60 17 16

- No.: 1210
- Timestamp: 20:44:06:591_0
- RFN: 3100
- Chip: 5632
- Event: Cancel Timer
- Source: ts_GMM_IdleUpdated:lt_HandleAttachRequest LINE 10
- Message Structure:
no details available
- Constraint:
t_WaitS
- BinaryMessage:

- No.: 1247
- Timestamp: 20:44:06:624_0
- RFN: 3103
- Chip: 16640
- Event: Send
- PCO: Dc
- Message: RRC_DataReq
- Source: ts_GMM_Authentication LINE 2
- Message Structure:
RRC_DataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[-1] = -
. (SapId)sapId[1] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. AUTHENTICATIONANDCIPHERINGREQUEST
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)gMMProtocolDiscriminator[4] = '1000'B
. . (MsgType)msgType[8] = '00010010'B
. . IMEISVRequest
. . . (B1)spare1[1] = '0'B
. . . (B3)value[3] = '000'B
. . CiphAlgorithm
. . . (B1)spare1[1] = '0'B
. . . (B3)algorithm[3] = '001'B
. . AC_ReferenceNumber
. . . (B4)value[4] = '0011'B
. . ForceToStandby
. . . (B1)spare[1] = '0'B
. . . (B3)value[3] = '000'B
. . AuthenticationParamterRAND
. . . (IEI8)iei[8] = '00100001'B
. . . (BitStringType)randValue[128] = '01010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101'B
. . CiphKeySeqNum_tv
. . . (IEI4)iei[4] = '1000'B
. . . (B1)spare1[1] = '0'B
. . . (KeySeq)keySeq[3] = '000'B
. . GMM_AUTN
. . . (IEI8)iei[8] = '00101000'B
. . . (Length)iel[1] = '10'O
. . . (BitStringType)aUTN[128] = '01010110010100010101000001010011010100100101110100000000000000000101010101010100010101110101011001010001010100000101001101010010'B
- Constraint:
ca_PS_DataReq
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 08 12 01 30 21 55 55 55 55 55 55 55 55 55 55 55 55 55 55 55 55 80 28 10 56 51 50 53 52 5d 00 00 55 54 57 56 51 50 53 52

- No.: 1251
- Timestamp: 20:44:07:294_0
- RFN: 3170
- Chip: 19456
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_GMM_Authentication LINE 7
- Message Structure:
RRC_DataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. (START_Value)start[0] = -
. AUTHENTICATIONANDCIPHERINGRESPONSE
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)gMMProtocolDiscriminator[4] = '1000'B
. . (MsgType)msgType[8] = '00010011'B
. . (B4)spare4[4] = '0000'B
. . AC_ReferenceNumber
. . . (B4)value[4] = '0011'B
. . AuthRsp_tv
. . . (IEI8)iei[8] = '00100010'B
. . . (BitStringType)value[32] = '01010101010101000101011101010110'B
. . GMM_MS_Identity
. . AuthRspExt
- Constraint:
car_PS_UplinkDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 08 13 03 22 55 54 57 56

- No.: 1254
- Timestamp: 20:44:07:297_1
- RFN: 3170
- Chip: 30976
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_GMM_Authentication LINE 10
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1291
- Timestamp: 20:44:07:310_0
- RFN: 3172
- Chip: 3328
- Event: Send
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_REQ
- Source: ts_SS_DownloadSecurityKey:lt_DownloadKeyCRLC LINE 1
- Message Structure:
CRLC_SecurityMode_Config_REQ
. (IntegerType)cellId = -1
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity = 1
. . (BitStringType)startValue[20] = "00000000000000000000"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = '01010111010101100101000101010000010100110101001001011101010111000101111101011110010110010101100001011011010110100101010101010100'B
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CRLC_SecurityModeCfgReq
- BinaryMessage:
30 21 02 01 ff 30 1c 0a 01 01 03 04 04 00 00 00 03 11 00 57 56 51 50 53 52 5d 5c 5f 5e 59 58 5b 5a 55 54

- No.: 1292
- Timestamp: 20:44:07:312_0
- RFN: 3172
- Chip: 10496
- Event: Receive
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_CNF
- Source: ts_SS_DownloadSecurityKey:lt_DownloadKeyCRLC LINE 2
- Message Structure:
CRLC_SecurityMode_Config_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1299
- Timestamp: 20:44:07:315_0
- RFN: 3172
- Chip: 22784
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 1
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
. (IntegerType)count_I_LSB_UL = -
. (IntegerType)count_I_LSB_DL = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 00 02 01 00 02 01 00

- No.: 1300
- Timestamp: 20:44:07:317_0
- RFN: 3172
- Chip: 30208
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 2
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 00 02 01 00

- No.: 1301
- Timestamp: 20:44:07:319_0
- RFN: 3173
- Chip: 256
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 3
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. (IntegerType)count_I_LSB_UL = -
. (IntegerType)count_I_LSB_DL = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 01 02 01 00

- No.: 1302
- Timestamp: 20:44:07:321_0
- RFN: 3173
- Chip: 7168
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 4
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 1303
- Timestamp: 20:44:07:323_0
- RFN: 3173
- Chip: 14336
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 5
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. (IntegerType)count_I_LSB_UL = -
. (IntegerType)count_I_LSB_DL = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 02 02 01 00

- No.: 1304
- Timestamp: 20:44:07:325_0
- RFN: 3173
- Chip: 21504
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 6
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 1305
- Timestamp: 20:44:07:327_0
- RFN: 3173
- Chip: 28416
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 7
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
. (IntegerType)count_I_LSB_UL = -
. (IntegerType)count_I_LSB_DL = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 03 02 01 00

- No.: 1306
- Timestamp: 20:44:07:328_0
- RFN: 3173
- Chip: 35840
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 8
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 1307
- Timestamp: 20:44:07:330_0
- RFN: 3174
- Chip: 4352
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 9
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
. (IntegerType)count_I_LSB_UL = -
. (IntegerType)count_I_LSB_DL = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 04 02 01 00

- No.: 1308
- Timestamp: 20:44:07:332_0
- RFN: 3174
- Chip: 11264
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 10
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 1312
- Timestamp: 20:44:07:335_0
- RFN: 3174
- Chip: 22016
- Event: Send
- PCO: CRLC
- Message: CRLC_Integrity_Activate_REQ
- Source: ts_CRLC_DL_Integrity LINE 1
- Message Structure:
CRLC_Integrity_Activate_REQ
. (IntegerType)cellId = -1
. (CN_DomainIdentity)cn_DomainIdentity = 1
. IntegrityActivationInfo
. . IntegrityProtectionModeInfo
. . . IntegrityProtectionModeCommand
. . . . startIntegrityProtection
. . . . . (BitStringType)integrityProtInitNumber[32] = "00000000000000000000000000000001"
. . . (IntegrityProtectionAlgorithm)integrityProtectionAlgorithm = 0
- Constraint:
ca_CRLC_DL_IntegrityActivateReq
- BinaryMessage:
30 15 02 01 ff 0a 01 01 30 0d 30 30 07 03 05 00 00 00 00 01 0a 01 00

- No.: 1313
- Timestamp: 20:44:07:336_0
- RFN: 3174
- Chip: 28416
- Event: Receive
- PCO: CRLC
- Message: CRLC_Integrity_Activate_CNF
- Source: ts_CRLC_DL_Integrity LINE 2
- Message Structure:
CRLC_Integrity_Activate_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_IntegrityActivateCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1320
- Timestamp: 20:44:07:340_0
- RFN: 3175
- Chip: 5120
- Event: Send
- PCO: CRLC
- Message: CRLC_Integrity_Activate_REQ
- Source: ts_RB2_UL_IntegrityActivate LINE 1
- Message Structure:
CRLC_Integrity_Activate_REQ
. (IntegerType)cellId = -1
. (CN_DomainIdentity)cn_DomainIdentity = 1
. IntegrityActivationInfo
. . IntegrityProtActivationInfoList
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity = 2
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
- Constraint:
ca_CRLC_UL_IntegrityActivateReq
- BinaryMessage:
30 10 02 01 ff 0a 01 01 30 08 30 06 02 01 02 02 01 00

- No.: 1321
- Timestamp: 20:44:07:342_0
- RFN: 3175
- Chip: 11008
- Event: Receive
- PCO: CRLC
- Message: CRLC_Integrity_Activate_CNF
- Source: ts_RB2_UL_IntegrityActivate LINE 2
- Message Structure:
CRLC_Integrity_Activate_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_IntegrityActivateCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1327
- Timestamp: 20:44:07:348_0
- RFN: 3175
- Chip: 35328
- Event: Send
- PCO: AM
- Message: RLC_AM_DATA_REQ
- Source: ts_RRC_Security:lt_SendSecurityModeCommand LINE 7
- Message Structure:
RLC_AM_DATA_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. AmConfirmationRequest
. aM_message
. . DL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00000000000000000000000000000000"
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . DL_DCCH_MessageType
. . . . SecurityModeCommand
. . . . . r3
. . . . . . SecurityModeCommand_r3_IEs
. . . . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . . . SecurityCapability
. . . . . . . . (BitStringType)cipheringAlgorithmCap[16] = '0000000000000011'B
. . . . . . . . (BitStringType)integrityProtectionAlgorithmCap[16] = '0000000000000010'B
. . . . . . . CipheringModeInfo
. . . . . . . IntegrityProtectionModeInfo
. . . . . . . . IntegrityProtectionModeCommand
. . . . . . . . . startIntegrityProtection
. . . . . . . . . . (BitStringType)integrityProtInitNumber[32] = "00000000000000000000000000000001"
. . . . . . . . (IntegrityProtectionAlgorithm)integrityProtectionAlgorithm = 0
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity = 1
. . . . . . . InterRAT_UE_SecurityCapList
. . . . . . laterNonCriticalExtensions
- Constraint:
cas_RRC_SecModeCmd
- BinaryMessage:
30 17 02 01 ff 02 01 02 05 00 80 00 00 00 04 04 00 01 80 01 40 00 00 00 30

- No.: 1333
- Timestamp: 20:44:07:473_0
- RFN: 3188
- Chip: 12800
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_IND
- Source: ts_RRC_Security:lt_StartSecurity_UE LINE 8
- Message Structure:
RLC_AM_DATA_IND
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. IntegrityResult
. . (IntegrityStatus)integrityUsed = 0
. aM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "10000001100000001110110111011101"
. . . . (IntegerType)rrc_MessageSequenceNumber = 1
. . . UL_DCCH_MessageType
. . . . SecurityModeComplete
. . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . IntegrityProtActivationInfo
. . . . . . RRC_MessageSequenceNumberList
. . . . . . . (IntegerType)_elem = 0
. . . . . . . (IntegerType)_elem = 0
. . . . . . . (IntegerType)_elem = 0
. . . . . . . (IntegerType)_elem = 0
. . . . . . . (IntegerType)_elem = 0
. . . . . laterNonCriticalExtensions
. . . . . . (BitStringType)securityModeComplete_r3_add_ext = 0
. . . . . . nonCriticalExtensions
- Constraint:
car_RRC_SecModeCmpl
- BinaryMessage:
30 12 02 01 ff 02 01 02 0a 01 00 c0 c0 76 ee 8d 21 00 00 00

- No.: 1334
- Timestamp: 20:44:07:474_0
- RFN: 3188
- Chip: 16896
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_Security:lt_StartSecurity_UE LINE 8
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1336
- Timestamp: 20:44:07:478_0
- RFN: 3188
- Chip: 31488
- Event: Send
- PCO: CRLC
- Message: CRLC_Integrity_Activate_REQ
- Source: ts_CRLC_UL_Integrity LINE 1
- Message Structure:
CRLC_Integrity_Activate_REQ
. (IntegerType)cellId = -1
. (CN_DomainIdentity)cn_DomainIdentity = 1
. IntegrityActivationInfo
. . IntegrityProtActivationInfoList
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity = 0
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity = 1
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity = 3
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity = 4
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
- Constraint:
ca_CRLC_UL_IntegrityActivateReq
- BinaryMessage:
30 28 02 01 ff 0a 01 01 30 20 30 06 02 01 00 02 01 00 30 06 02 01 01 02 01 00 30 06 02 01 03 02 01 00 30 06 02 01 04 02 01 00

- No.: 1337
- Timestamp: 20:44:07:480_0
- RFN: 3189
- Chip: 1536
- Event: Receive
- PCO: CRLC
- Message: CRLC_Integrity_Activate_CNF
- Source: ts_CRLC_UL_Integrity LINE 2
- Message Structure:
CRLC_Integrity_Activate_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_IntegrityActivateCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1347
- Timestamp: 20:44:07:498_0
- RFN: 3190
- Chip: 33792
- Event: Send
- PCO: Dc
- Message: RRC_DataReq
- Source: ts_GMM_IdleUpdated:lt_AttachAccept LINE 12
- Message Structure:
RRC_DataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[-1] = -
. (SapId)sapId[1] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. ATTACHACCEPT
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)gMMProtocolDiscriminator[4] = '1000'B
. . (MsgType)msgType[8] = '00000010'B
. . ForceToStandby
. . . (B1)spare[1] = '0'B
. . . (B3)value[3] = '000'B
. . AttachResult
. . . (B1)spare[1] = '0'B
. . . (B3)result[3] = '001'B
. . GPRS_Timer_v
. . . (B3)unit[3] = '111'B
. . . (B5)value[5] = '00000'B
. . (B4)spare[4] = '0000'B
. . RadioPriority_v
. . . (B1)spare[1] = '0'B
. . . (B3)value[3] = '100'B
. . RAI_v
. . . (OctetStringType)plmn[3] = '00F110'O
. . . (OctetStringType)lac[2] = '0001'O
. . . (OctetStringType)rac[1] = '05'O
. . PTMSI_Signature
. . . (IEI8)iei[8] = '00011001'B
. . . (OctetStringType)value[3] = 'AB1234'O
. . GPRS_Timer
. . GMM_MS_IdentityPTMSI
. . . (IEI8)iei[8] = '00011000'B
. . . (Length)iel[1] = '05'O
. . . (B4)iDigit1[4] = '1111'B
. . . (B1)oddEvenInd[1] = '0'B
. . . (B3)typeOfId[3] = '100'B
. . . (OctetStringType)otherDigits[-1] = '12345678'O
. . GMM_MS_Identity
. . GMM_Cause
. . GPRS_Timer
. . CellNotification
. . PLMN_List
- Constraint:
ca_PS_DataReq
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 08 02 01 e0 04 00 f1 10 00 01 05 19 ab 12 34 18 05 f4 12 34 56 78

- No.: 1351
- Timestamp: 20:44:07:641_0
- RFN: 3205
- Chip: 6144
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_GMM_IdleUpdated:lt_AttachAccept LINE 13
- Message Structure:
RRC_DataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. (START_Value)start[0] = -
. ATTACHCOMPLETE
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)gMMProtocolDiscriminator[4] = '1000'B
. . (MsgType)msgType[8] = '00000011'B
- Constraint:
car_PS_UplinkDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 08 03

- No.: 1362
- Timestamp: 20:44:07:644_2
- RFN: 3205
- Chip: 19200
- Event: Start Timer
- Source: ts_RRC_Delay LINE 1
- Message Structure:
no details available
- Constraint:
t_Dly (1000 Ms)
- BinaryMessage:

- No.: 1366
- Timestamp: 20:44:08:636_0
- RFN: 3304
- Chip: 23552
- Event: Timeout
- Source: ts_RRC_Delay LINE 2
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 1371
- Timestamp: 20:44:08:641_0
- RFN: 3305
- Chip: 4096
- Event: Send
- PCO: UM
- Message: RLC_UM_DATA_REQ
- Source: ts_RRC_ConnRel:lt_Send_RRC_ConnectionRelease LINE 3
- Message Structure:
RLC_UM_DATA_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. uM_message
. . DL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00000000000000000000000000000000"
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . DL_DCCH_MessageType
. . . . RRCConnectionRelease
. . . . . r3
. . . . . . RRCConnectionRelease_r3_IEs
. . . . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . . . (IntegerType)n_308 = 1
. . . . . . . (ReleaseCause)releaseCause = 0
. . . . . . . Rplmn_Information
. . . . . . laterNonCriticalExtensions
. (BooleanType)specialLI = FALSE
- Constraint:
cas_RRC_ConnRelDCCH
- BinaryMessage:
30 10 02 01 ff 02 01 01 80 00 00 00 03 c8 00 01 01 00

- No.: 1375
- Timestamp: 20:44:08:772_0
- RFN: 3318
- Chip: 8192
- Event: Receive
- PCO: UM
- Message: RLC_UM_DATA_IND
- Source: ts_RRC_ConnRel:lt_Send_RRC_ConnectionRelease LINE 4
- Message Structure:
RLC_UM_DATA_IND
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. IntegrityResult
. uM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "10101101101011101001000000111001"
. . . . (IntegerType)rrc_MessageSequenceNumber = 1
. . . UL_DCCH_MessageType
. . . . RRCConnectionReleaseComplete
. . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . FailureCauseWithProtErr
. . . . . laterNonCriticalExtensions
. . . . . . (BitStringType)rrcConnectionReleaseComplete_r3_add_ext = 0
. . . . . . nonCriticalExtensions
- Constraint:
car_RRC_ConnRelCmplUM
- BinaryMessage:
30 0c 02 01 ff 02 01 01 d6 d7 48 1c 8c 40

- No.: 1376
- Timestamp: 20:44:08:773_0
- RFN: 3318
- Chip: 12032
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ConnRel:lt_Send_RRC_ConnectionRelease LINE 4
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1379
- Timestamp: 20:44:08:774_1
- RFN: 3318
- Chip: 17408
- Event: Start Timer
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 1
- Message Structure:
no details available
- Constraint:
t_Dly (5000 Ms)
- BinaryMessage:

- No.: 1383
- Timestamp: 20:44:08:921_0
- RFN: 3333
- Chip: 8448
- Event: Receive
- PCO: UM
- Message: RLC_UM_DATA_IND
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 4
- Message Structure:
RLC_UM_DATA_IND
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. IntegrityResult
. uM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00011100010101000111110101101001"
. . . . (IntegerType)rrc_MessageSequenceNumber = 2
. . . UL_DCCH_MessageType
. . . . RRCConnectionReleaseComplete
. . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . FailureCauseWithProtErr
. . . . . laterNonCriticalExtensions
. . . . . . (BitStringType)rrcConnectionReleaseComplete_r3_add_ext = 0
. . . . . . nonCriticalExtensions
- Constraint:
car_RRC_ConnRelCmplUM
- BinaryMessage:
30 0c 02 01 ff 02 01 01 8e 2a 3e b4 94 40

- No.: 1384
- Timestamp: 20:44:08:922_0
- RFN: 3333
- Chip: 12288
- Event: Cancel Timer
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 4
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 1385
- Timestamp: 20:44:08:922_1
- RFN: 3333
- Chip: 13824
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 4
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1391
- Timestamp: 20:44:08:927_0
- RFN: 3333
- Chip: 28160
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 01 0a 01 00 05 00

- No.: 1395
- Timestamp: 20:44:08:934_0
- RFN: 3334
- Chip: 13824
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 1398
- Timestamp: 20:44:08:937_0
- RFN: 3334
- Chip: 25344
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 02 0a 01 00 05 00

- No.: 1402
- Timestamp: 20:44:08:944_0
- RFN: 3335
- Chip: 15104
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 1405
- Timestamp: 20:44:08:947_0
- RFN: 3335
- Chip: 26368
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 03 0a 01 00 05 00

- No.: 1409
- Timestamp: 20:44:08:954_0
- RFN: 3336
- Chip: 15104
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 1412
- Timestamp: 20:44:08:957_0
- RFN: 3336
- Chip: 25344
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 04 0a 01 00 05 00

- No.: 1416
- Timestamp: 20:44:08:968_0
- RFN: 3337
- Chip: 32768
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 1419
- Timestamp: 20:44:08:976_0
- RFN: 3338
- Chip: 24320
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 136
. . . . . UL_RLC_Mode
. . . . . . UL_UM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (NoExplicitDiscard)timerBasedNoExplicit = 9
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = 1
. . . . (IntegerType)dLlogicalChannelIdentity = 1
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_UM_Info
- BinaryMessage:
30 22 02 01 ff 02 01 01 0a 01 00 30 17 30 0d 05 00 30 09 02 02 00 88 30 03 0a 01 09 30 06 02 01 01 02 01 01

- No.: 1423
- Timestamp: 20:44:08:988_0
- RFN: 3339
- Chip: 30464
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 1424
- Timestamp: 20:44:08:996_0
- RFN: 3340
- Chip: 24576
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 3
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . (TimerEPC)timerEPC = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . (TimerRST)timerRST = 9
. . . . . . . (MaxRST)max_RST = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = 2
. . . . (IntegerType)dLlogicalChannelIdentity = 2
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 02 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 27 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 02 02 01 02

- No.: 1428
- Timestamp: 20:44:09:017_0
- RFN: 3342
- Chip: 27392
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 4
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 1429
- Timestamp: 20:44:09:026_0
- RFN: 3343
- Chip: 23040
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 5
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . (TimerEPC)timerEPC = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . (TimerRST)timerRST = 9
. . . . . . . (MaxRST)max_RST = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = 3
. . . . (IntegerType)dLlogicalChannelIdentity = 3
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 03 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 27 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 03 02 01 03

- No.: 1433
- Timestamp: 20:44:09:048_0
- RFN: 3345
- Chip: 31744
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 6
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 1434
- Timestamp: 20:44:09:057_0
- RFN: 3346
- Chip: 27136
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 7
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . (TimerEPC)timerEPC = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . (TimerRST)timerRST = 9
. . . . . . . (MaxRST)max_RST = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = 4
. . . . (IntegerType)dLlogicalChannelIdentity = 4
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 04 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 27 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 04 02 01 04

- No.: 1438
- Timestamp: 20:44:09:079_0
- RFN: 3348
- Chip: 37632
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 8
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 1480
- Timestamp: 20:44:09:105_0
- RFN: 3351
- Chip: 20224
- Event: Start Timer
- Source: ts_RRC_Delay LINE 1
- Message Structure:
no details available
- Constraint:
t_Dly (5000 Ms)
- BinaryMessage:

- No.: 1482
- Timestamp: 20:44:09:107_0
- RFN: 3351
- Chip: 30720
- Event: Receive
- PCO: CPHY
- Message: CPHY_Out_of_Sync_IND
- Source: RRC_Def1 LINE 15
- Message Structure:
CPHY_Out_of_Sync_IND
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_OutOfSyncInd
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 1483
- Timestamp: 20:44:09:108_0
- RFN: 3351
- Chip: 32512
- Event: Cancel Timer
- Source: RRC_Def1 LINE 15
- Message Structure:
no details available
- Constraint:
t_T312
- BinaryMessage:

- No.: 1484
- Timestamp: 20:44:09:108_1
- RFN: 3351
- Chip: 34816
- Event: Default
- Source: RRC_Def1 LINE 0
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1485
- Timestamp: 20:44:09:109_0
- RFN: 3351
- Chip: 35584
- Event: Default
- Source: ts_RRC_Delay LINE 2
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1490
- Timestamp: 20:44:14:091_0
- RFN: 3850
- Chip: 6144
- Event: Timeout
- Source: ts_RRC_Delay LINE 2
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 1503
- Timestamp: 20:44:14:118_0
- RFN: 3852
- Chip: 33280
- Event: Send
- PCO: CMAC
- Message: CMAC_PAGING_Config_REQ
- Source: ts_CMAC_Pag1_Cfg LINE 4
- Message Structure:
CMAC_PAGING_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 5
. (RatType)ratType = 0
. CmacPagingConfigReq
. . pI_BitMapInfo
. . . (BitStringType)e18[18] = '010000000000000000'B
. . (IntegerType)dRX_CycleLength = 7
. . IMSI_GSM_MAP
. . . (IntegerType)_elem = 0
. . . (IntegerType)_elem = 0
. . . (IntegerType)_elem = 1
. . . (IntegerType)_elem = 0
. . . (IntegerType)_elem = 1
. . . (IntegerType)_elem = 0
. . . (IntegerType)_elem = 1
. . . (IntegerType)_elem = 2
. . . (IntegerType)_elem = 3
. . . (IntegerType)_elem = 4
. . . (IntegerType)_elem = 5
. . . (IntegerType)_elem = 6
. . . (IntegerType)_elem = 0
. . . (IntegerType)_elem = 6
. . . (IntegerType)_elem = 3
. . (BooleanType)t_pich_T_sccpch = FALSE
- Constraint:
ca_CMAC_PagingCfgReq
- BinaryMessage:
30 46 02 01 00 02 01 05 0a 01 00 30 3b 03 04 06 40 00 00 02 01 07 30 2d 02 01 00 02 01 00 02 01 01 02 01 00 02 01 01 02 01 00 02 01 01 02 01 02 02 01 03 02 01 04 02 01 05 02 01 06 02 01 00 02 01 06 02 01 03 01 01 00

- No.: 1507
- Timestamp: 20:44:14:124_0
- RFN: 3853
- Chip: 16128
- Event: Receive
- PCO: CMAC
- Message: CMAC_PAGING_Config_CNF
- Source: ts_CMAC_Pag1_Cfg LINE 5
- Message Structure:
CMAC_PAGING_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 5
- Constraint:
ca_CMAC_PagingCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 05

- No.: 1509
- Timestamp: 20:44:14:147_0
- RFN: 3855
- Chip: 29952
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_RRC_ConnEst_DCH_MT_PTMSI LINE 5
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -2
. tM_message
. . PCCH_Message
. . . PCCH_MessageType
. . . . PagingType1
. . . . . PagingRecordList
. . . . . . PagingRecord
. . . . . . . cn_Identity
. . . . . . . . (PagingCause)pagingCause = 2
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = 1
. . . . . . . . CN_PagedUE_Identity
. . . . . . . . . (BitStringType)p_TMSI_GSM_MAP[32] = "00010010001101000101011001111000"
. . . . . BCCH_ModificationInfo
. . . . . laterNonCriticalExtensions
- Constraint:
cas_PagingType1
- BinaryMessage:
30 0c 02 01 00 02 01 fe 40 54 24 68 ac f0

- No.: 1513
- Timestamp: 20:44:14:879_0
- RFN: 3928
- Chip: 37632
- Event: Receive
- PCO: TM
- Message: RLC_TR_DATA_IND
- Source: ts_RRC_ConnEst_DCH_MT_PTMSI LINE 6
- Message Structure:
RLC_TR_DATA_IND
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
. tM_message
. . UL_CCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode = 0
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . UL_CCCH_MessageType
. . . . RRCConnectionRequest
. . . . . InitialUE_Identity
. . . . . . TMSI_and_LAI_GSM_MAP
. . . . . . . (BitStringType)tmsi[32] = "00010010001101000101011001111000"
. . . . . . . LAI
. . . . . . . . PLMN_Identity
. . . . . . . . . MCC
. . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . (IntegerType)_elem = 1
. . . . . . . . . MNC
. . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . (IntegerType)_elem = 1
. . . . . . . . (BitStringType)lac[16] = '0000000000000001'B
. . . . . (EstablishmentCause)establishmentCause = 7
. . . . . (ProtocolErrorIndicator)protocolErrorIndicator = 0
. . . . . MeasuredResultsOnRACH
. . . . . . currentCell
. . . . . . . modeSpecificInfo
. . . . . . . . fdd
. . . . . . . . . measurementQuantity
. . . . . . . . . . (IntegerType)cpich_Ec_N0 = 0
. . . . . v3d0NonCriticalExtensions
. . . . . . RRCConnectionRequest_v3d0ext_IEs
. . . . . . . (BitStringType)uESpecificBehaviourInformation1idle = 0
. . . . . . nonCriticalExtensions
- Constraint:
car_RRC_ConnReq
- BinaryMessage:
30 11 02 01 00 02 01 00 21 12 34 56 78 00 10 08 00 09 c0

- No.: 1514
- Timestamp: 20:44:14:943_0
- RFN: 3935
- Chip: 13312
- Event: Send
- PCO: UM
- Message: RLC_UM_DATA_REQ
- Source: ts_RRC_ConnEst_DCH_MT_PTMSI LINE 7
- Message Structure:
RLC_UM_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
. uM_message
. . DL_CCCH_Message
. . . IntegrityCheckInfo
. . . DL_CCCH_MessageType
. . . . RRCConnectionSetup
. . . . . r3
. . . . . . RRCConnectionSetup_r3_IEs
. . . . . . . InitialUE_Identity
. . . . . . . . TMSI_and_LAI_GSM_MAP
. . . . . . . . . (BitStringType)tmsi[32] = "00010010001101000101011001111000"
. . . . . . . . . LAI
. . . . . . . . . . PLMN_Identity
. . . . . . . . . . . MCC
. . . . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . . . (IntegerType)_elem = 1
. . . . . . . . . . . MNC
. . . . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . . . (IntegerType)_elem = 1
. . . . . . . . . . (BitStringType)lac[16] = '0000000000000001'B
. . . . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . . . (IntegerType)activationTime = -
. . . . . . . U_RNTI
. . . . . . . . (BitStringType)srnc_Identity[12] = "000000000001"
. . . . . . . . (BitStringType)s_RNTI[20] = "00000000000000000001"
. . . . . . . (BitStringType)new_c_RNTI[16] = -
. . . . . . . (RRC_StateIndicator)rrc_StateIndicator = 0
. . . . . . . (IntegerType)utran_DRX_CycleLengthCoeff = 9
. . . . . . . CapabilityUpdateRequirement
. . . . . . . . (BooleanType)ue_RadioCapabilityFDDUpdateRequirement = TRUE
. . . . . . . . (BooleanType)ue_RadioCapabilityTDDUpdateRequirement = FALSE
. . . . . . . . SystemSpecificCapUpdateReqList
. . . . . . . . . (SystemSpecificCapUpdateReq)_elem = 0
. . . . . . . SRB_InformationSetupList2
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_UM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 1
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 1
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . . . . . . . (TimerRST)timerRST = 9
. . . . . . . . . . . . . (MaxRST)max_RST = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 2
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 2
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . . . . . . . (TimerRST)timerRST = 9
. . . . . . . . . . . . . (MaxRST)max_RST = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 3
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 3
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . . . . . . . (TimerRST)timerRST = 9
. . . . . . . . . . . . . (MaxRST)max_RST = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 4
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 4
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . UL_CommonTransChInfo
. . . . . . . . TFC_Subset
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . TFCS
. . . . . . . . . . . ExplicitTFCS_Configuration
. . . . . . . . . . . . TFCS_ReconfAdd
. . . . . . . . . . . . . ctfcSize
. . . . . . . . . . . . . . ctfc2Bit
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . . . . . . . (IntegerType)ctfc2 = 0
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . . . . . . . (IntegerType)ctfc2 = 1
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 11
. . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . UL_AddReconfTransChInfoList
. . . . . . . . UL_AddReconfTransChInformation
. . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType = 0
. . . . . . . . . (IntegerType)transportChannelIdentity = 5
. . . . . . . . . TransportFormatSet
. . . . . . . . . . DedicatedTransChTFS
. . . . . . . . . . . tti
. . . . . . . . . . . . DedicatedDynamicTF_InfoList
. . . . . . . . . . . . . DedicatedDynamicTF_Info
. . . . . . . . . . . . . . rlc_Size
. . . . . . . . . . . . . . . BitModeRLC_SizeInfo
. . . . . . . . . . . . . . . . sizeType2
. . . . . . . . . . . . . . . . . (IntegerType)part1 = 2
. . . . . . . . . . . . . . . . . (IntegerType)part2 = -
. . . . . . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . LogicalChannelList
. . . . . . . . . . . SemistaticTF_Information
. . . . . . . . . . . . ChannelCodingType
. . . . . . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . . . . . (IntegerType)rateMatchingAttribute = 192
. . . . . . . . . . . . (CRC_Size)crc_Size = 3
. . . . . . . DL_CommonTransChInfo
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . dl_Parameters
. . . . . . . DL_AddReconfTransChInfoList
. . . . . . . . DL_AddReconfTransChInformation
. . . . . . . . . (DL_TrCH_Type)dl_TransportChannelType = 0
. . . . . . . . . (IntegerType)dl_transportChannelIdentity = 10
. . . . . . . . . tfs_SignallingMode
. . . . . . . . . . UL_TransportChannelIdentity
. . . . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType = 0
. . . . . . . . . . . (IntegerType)ul_TransportChannelIdentity = 5
. . . . . . . . . QualityTarget
. . . . . . . . . . (IntegerType)bler_QualityValue = -20
. . . . . . . . . TM_SignallingInfo
. . . . . . . FrequencyInfo
. . . . . . . (IntegerType)maxAllowedUL_TX_Power = -
. . . . . . . UL_ChannelRequirement
. . . . . . . . UL_DPCH_Info
. . . . . . . . . UL_DPCH_PowerControlInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (IntegerType)dpcch_PowerOffset = -40
. . . . . . . . . . . (IntegerType)pc_Preamble = 1
. . . . . . . . . . . (IntegerType)sRB_delay = 7
. . . . . . . . . . . PowerControlAlgorithm
. . . . . . . . . . . . (IntegerType)algorithm1 = 1
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (ScramblingCodeType)scramblingCodeType = 1
. . . . . . . . . . . (IntegerType)scramblingCode = 0
. . . . . . . . . . . (IntegerType)numberOfDPDCH = -
. . . . . . . . . . . (SpreadingFactor)spreadingFactor = 4
. . . . . . . . . . . (BooleanType)tfci_Existence = TRUE
. . . . . . . . . . . (IntegerType)numberOfFBI_Bits = -
. . . . . . . . . . . (PuncturingLimit)puncturingLimit = 15
. . . . . . . DL_CommonInformation
. . . . . . . . DL_DPCH_InfoCommon
. . . . . . . . . cfnHandling
. . . . . . . . . . initialise
. . . . . . . . . . . (IntegerType)cfntargetsfnframeoffset = -
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . DL_DPCH_PowerControlInfo
. . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . (DPC_Mode)dpc_Mode = 0
. . . . . . . . . . . (IntegerType)powerOffsetPilot_pdpdch = 0
. . . . . . . . . . . Dl_rate_matching_restriction
. . . . . . . . . . . SF512_AndPilot
. . . . . . . . . . . . (PilotBits128)sfd128 = 0
. . . . . . . . . . . (PositionFixedOrFlexible)positionFixedOrFlexible = 0
. . . . . . . . . . . (BooleanType)tfci_Existence = FALSE
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . (IntegerType)defaultDPCH_OffsetValue = 0
. . . . . . . . . . DPCH_CompressedModeInfo
. . . . . . . . . . (TX_DiversityMode)tx_DiversityMode = 0
. . . . . . . . . . SSDT_Information
. . . . . . . DL_InformationPerRL_List
. . . . . . . . DL_InformationPerRL
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . PrimaryCPICH_Info
. . . . . . . . . . . . (IntegerType)primaryScramblingCode = 100
. . . . . . . . . . . PDSCH_SHO_DCH_Info
. . . . . . . . . . . PDSCH_CodeMapping
. . . . . . . . . DL_DPCH_InfoPerRL
. . . . . . . . . . fdd
. . . . . . . . . . . (PCPICH_UsageForChannelEst)pCPICH_UsageForChannelEst = 0
. . . . . . . . . . . (IntegerType)dpch_FrameOffset = 0
. . . . . . . . . . . SecondaryCPICH_Info
. . . . . . . . . . . DL_ChannelisationCodeList
. . . . . . . . . . . . DL_ChannelisationCode
. . . . . . . . . . . . . (IntegerType)secondaryScramblingCode = 1
. . . . . . . . . . . . . SF512_AndCodeNumber
. . . . . . . . . . . . . . (IntegerType)sf128 = 0
. . . . . . . . . . . . . (ScramblingCodeChange)scramblingCodeChange = 1
. . . . . . . . . . . (IntegerType)tpc_CombinationIndex = 0
. . . . . . . . . . . (SSDT_CellIdentity)ssdt_CellIdentity = -
. . . . . . . . . . . (ClosedLoopTimingAdjMode)closedLoopTimingAdjMode = -
. . . . . . . . . SCCPCH_InfoForFACH
. . . . . . laterNonCriticalExtensions
. (BooleanType)specialLI = TRUE
- Constraint:
cas_RRC_ConnSetup
- BinaryMessage:
30 78 02 01 00 02 01 00 30 e7 22 46 8a cf 00 02 01 00 01 00 04 00 00 4d 82 69 3a 10 10 89 0d 42 00 02 81 9e 8e 46 c9 ce 7c 9c 4e 74 20 a5 12 3a 8c 00 15 13 3d 1c 8d 93 9c f9 38 9c e8 42 52 24 b5 28 00 4a 46 7a 39 1b 27 39 f2 71 39 d0 86 b4 49 ea 70 00 d4 c8 00 06 25 2b f0 02 00 08 82 23 bf 66 08 98 95 a5 47 a2 00 00 01 3f 90 0a 14 00 02 06 40 00 0c 28 08 01 01 ff

- No.: 1522
- Timestamp: 20:44:14:984_1
- RFN: 3939
- Chip: 16896
- Event: Start Timer
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 3
- Message Structure:
no details available
- Constraint:
t_WaitMS (13500 Ms)
- BinaryMessage:

- No.: 1527
- Timestamp: 20:44:15:228_0
- RFN: 3963
- Chip: 31488
- Event: Receive
- PCO: CPHY
- Message: CPHY_Sync_IND
- Source: RRC_Def1 LINE 13
- Message Structure:
CPHY_Sync_IND
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_SyncInd
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 1528
- Timestamp: 20:44:15:229_0
- RFN: 3963
- Chip: 33536
- Event: Cancel Timer
- Source: RRC_Def1 LINE 13
- Message Structure:
no details available
- Constraint:
t_T312
- BinaryMessage:

- No.: 1529
- Timestamp: 20:44:15:229_1
- RFN: 3963
- Chip: 35328
- Event: Default
- Source: RRC_Def1 LINE 0
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1530
- Timestamp: 20:44:15:229_2
- RFN: 3963
- Chip: 36096
- Event: Default
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1535
- Timestamp: 20:44:15:343_0
- RFN: 3975
- Chip: 12288
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_IND
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
RLC_AM_DATA_IND
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. IntegrityResult
. . (IntegrityStatus)integrityUsed = 0
. aM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode = 0
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . UL_DCCH_MessageType
. . . . RRCConnectionSetupComplete
. . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . STARTList
. . . . . . STARTSingle
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity = 1
. . . . . . . (BitStringType)start_Value[20] = "00000000000000000010"
. . . . . . STARTSingle
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity = 0
. . . . . . . (BitStringType)start_Value[20] = "00000000000000000010"
. . . . . UE_RadioAccessCapability
. . . . . . (AccessStratumReleaseIndicator)accessStratumReleaseIndicator = 0
. . . . . . PDCP_Capability
. . . . . . . (BooleanType)losslessSRNS_RelocationSupport = FALSE
. . . . . . . supportForRfc2507
. . . . . . RLC_Capability
. . . . . . . (TotalRLC_AM_BufferSize)totalRLC_AM_BufferSize = 2
. . . . . . . (MaximumRLC_WindowSize)maximumRLC_WindowSize = 0
. . . . . . . (MaximumAM_EntityNumberRLC_Cap)maximumAM_EntityNumber = 3
. . . . . . TransportChannelCapability
. . . . . . . DL_TransChCapability
. . . . . . . . (MaxNoBits)maxNoBitsReceived = 4
. . . . . . . . (MaxNoBits)maxConvCodeBitsReceived = 1
. . . . . . . . TurboSupport
. . . . . . . . . (MaxNoBits)supported = 4
. . . . . . . . (MaxSimultaneousTransChsDL)maxSimultaneousTransChs = 1
. . . . . . . . (IntegerType)maxSimultaneousCCTrCH_Count = 1
. . . . . . . . (MaxTransportBlocksDL)maxReceivedTransportBlocks = 2
. . . . . . . . (MaxNumberOfTFC_DL)maxNumberOfTFC = 4
. . . . . . . . (MaxNumberOfTF)maxNumberOfTF = 1
. . . . . . . UL_TransChCapability
. . . . . . . . (MaxNoBits)maxNoBitsTransmitted = 3
. . . . . . . . (MaxNoBits)maxConvCodeBitsTransmitted = 1
. . . . . . . . TurboSupport
. . . . . . . . . (MaxNoBits)supported = 3
. . . . . . . . (MaxSimultaneousTransChsUL)maxSimultaneousTransChs = 2
. . . . . . . . modeSpecificInfo
. . . . . . . . (MaxTransportBlocksUL)maxTransmittedBlocks = 2
. . . . . . . . (MaxNumberOfTFC_UL)maxNumberOfTFC = 3
. . . . . . . . (MaxNumberOfTF)maxNumberOfTF = 0
. . . . . . RF_Capability
. . . . . . . fddRF_Capability
. . . . . . . . (IntegerType)ue_PowerClass = 4
. . . . . . . . (TxRxFrequencySeparation)txRxFrequencySeparation = 0
. . . . . . . tddRF_Capability
. . . . . . . . (IntegerType)ue_PowerClass = 0
. . . . . . . . (RadioFrequencyBandTDDList)radioFrequencyTDDBandList = 0
. . . . . . . . (ChipRateCapability)chipRateCapability = 0
. . . . . . PhysicalChannelCapability
. . . . . . . fddPhysChCapability
. . . . . . . . DL_PhysChCapabilityFDD
. . . . . . . . . (IntegerType)maxNoDPCH_PDSCH_Codes = 3
. . . . . . . . . (MaxNoPhysChBitsReceived)maxNoPhysChBitsReceived = 6
. . . . . . . . . (BooleanType)supportForSF_512 = FALSE
. . . . . . . . . (BooleanType)supportOfPDSCH = FALSE
. . . . . . . . . SimultaneousSCCPCH_DPCH_Reception
. . . . . . . . UL_PhysChCapabilityFDD
. . . . . . . . . (MaxNoDPDCH_BitsTransmitted)maxNoDPDCH_BitsTransmitted = 2
. . . . . . . . . (BooleanType)supportOfPCPCH = FALSE
. . . . . . . tddPhysChCapability
. . . . . . . . DL_PhysChCapabilityTDD
. . . . . . . . . (IntegerType)maxTS_PerFrame = 0
. . . . . . . . . (IntegerType)maxPhysChPerFrame = 0
. . . . . . . . . (MinimumSF_DL)minimumSF = 0
. . . . . . . . . (BooleanType)supportOfPDSCH = FALSE
. . . . . . . . . (IntegerType)maxPhysChPerTS = 0
. . . . . . . . UL_PhysChCapabilityTDD
. . . . . . . . . (IntegerType)maxTS_PerFrame = 0
. . . . . . . . . (MaxPhysChPerTimeslot)maxPhysChPerTimeslot = 0
. . . . . . . . . (MinimumSF_UL)minimumSF = 0
. . . . . . . . . (BooleanType)supportOfPUSCH = FALSE
. . . . . . UE_MultiModeRAT_Capability
. . . . . . . MultiRAT_Capability
. . . . . . . . (BooleanType)supportOfGSM = TRUE
. . . . . . . . (BooleanType)supportOfMulticarrier = FALSE
. . . . . . . (MultiModeCapability)multiModeCapability = 1
. . . . . . SecurityCapability
. . . . . . . (BitStringType)cipheringAlgorithmCap[16] = '0000000000000011'B
. . . . . . . (BitStringType)integrityProtectionAlgorithmCap[16] = '0000000000000010'B
. . . . . . UE_Positioning_Capability
. . . . . . . (BooleanType)standaloneLocMethodsSupported = FALSE
. . . . . . . (BooleanType)ue_BasedOTDOA_Supported = FALSE
. . . . . . . (NetworkAssistedGPS_Supported)networkAssistedGPS_Supported = 3
. . . . . . . (BooleanType)supportForUE_GPS_TimingOfCellFrames = FALSE
. . . . . . . (BooleanType)supportForIPDL = FALSE
. . . . . . MeasurementCapability
. . . . . . . CompressedModeMeasCapability
. . . . . . . . (BooleanType)fdd_Measurements = TRUE
. . . . . . . . (BooleanType)tdd_Measurements = FALSE
. . . . . . . . GSM_Measurements
. . . . . . . . . (BooleanType)gsm900 = TRUE
. . . . . . . . . (BooleanType)dcs1800 = TRUE
. . . . . . . . . (BooleanType)gsm1900 = FALSE
. . . . . . . . (BooleanType)multiCarrierMeasurements = FALSE
. . . . . . . CompressedModeMeasCapability
. . . . . . . . (BooleanType)fdd_Measurements = TRUE
. . . . . . . . (BooleanType)tdd_Measurements = FALSE
. . . . . . . . GSM_Measurements
. . . . . . . . . (BooleanType)gsm900 = TRUE
. . . . . . . . . (BooleanType)dcs1800 = TRUE
. . . . . . . . . (BooleanType)gsm1900 = FALSE
. . . . . . . . (BooleanType)multiCarrierMeasurements = FALSE
. . . . . v370NonCriticalExtensions
. . . . . . RRCConnectionSetupComplete_v370ext
. . . . . . . UE_RadioAccessCapability_v370ext
. . . . . . v380NonCriticalExtensions
. . . . . . . RRCConnectionSetupComplete_v380ext_IEs
. . . . . . . . UE_RadioAccessCapability_v380ext
. . . . . . . . . UE_PositioningCapabilityExt_v380
. . . . . . . . . . (BooleanType)rx_tx_TimeDifferenceType2Capable = FALSE
. . . . . . . . DL_PhysChCapabilityFDD_v380ext
. . . . . . . . . (SupportOfDedicatedPilotsForChEstimation)supportOfDedicatedPilotsForChEstimation = 0
. . . . . . . v3a0NonCriticalExtensions
. . . . . . . . RRCConnectionSetupComplete_v3a0ext_IEs
. . . . . . . . . UE_RadioAccessCapability_v3a0ext
. . . . . . . . . . UE_PositioningCapabilityExt_v3a0
. . . . . . . . . . . (UE_PositioningCapabilityExt_v3a0_list_0)validity_CellPCH_UraPCH = 0
. . . . . . . . laterNonCriticalExtensions
. . . . . . . . . (BitStringType)rrcConnectionSetupComplete_r3_add_ext = 0
. . . . . . . . . nonCriticalExtensions
- Constraint:
car_RRC_ConnSetupCmpl
- BinaryMessage:
30 27 02 01 ff 02 01 02 0a 05 01 00 00 00 00 4a 0c 00 00 80 00 05 11 a0 d1 04 84 c6 68 46 2c 93 02 48 00 18 00 11 8f 8f 80

- No.: 1536
- Timestamp: 20:44:15:353_0
- RFN: 3976
- Chip: 14080
- Event: Cancel Timer
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
t_WaitMS
- BinaryMessage:

- No.: 1537
- Timestamp: 20:44:15:353_1
- RFN: 3976
- Chip: 14848
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1551
- Timestamp: 20:44:15:360_0
- RFN: 3977
- Chip: 1024
- Event: Send
- PCO: CMAC
- Message: CMAC_SecurityMode_Config_REQ
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 1
- Message Structure:
CMAC_SecurityMode_Config_REQ
. (IntegerType)cellId = 0
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity = 1
. . (BitStringType)startValue[20] = "00000000000000000010"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = -
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CMAC_SecurityModeCfgReq
- BinaryMessage:
30 0e 02 01 00 30 09 0a 01 01 03 04 04 00 00 20

- No.: 1552
- Timestamp: 20:44:15:362_0
- RFN: 3977
- Chip: 7680
- Event: Receive
- PCO: CMAC
- Message: CMAC_SecurityMode_Config_CNF
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 2
- Message Structure:
CMAC_SecurityMode_Config_CNF
. (IntegerType)cellId = 0
- Constraint:
ca_CMAC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 00

- No.: 1553
- Timestamp: 20:44:15:363_0
- RFN: 3977
- Chip: 14848
- Event: Send
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_REQ
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 3
- Message Structure:
CRLC_SecurityMode_Config_REQ
. (IntegerType)cellId = -1
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity = 1
. . (BitStringType)startValue[20] = "00000000000000000010"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = -
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CRLC_SecurityModeCfgReq
- BinaryMessage:
30 0e 02 01 ff 30 09 0a 01 01 03 04 04 00 00 20

- No.: 1554
- Timestamp: 20:44:15:365_0
- RFN: 3977
- Chip: 21760
- Event: Receive
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_CNF
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 4
- Message Structure:
CRLC_SecurityMode_Config_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1568
- Timestamp: 20:44:15:371_0
- RFN: 3978
- Chip: 4096
- Event: Send
- PCO: CMAC
- Message: CMAC_SecurityMode_Config_REQ
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 1
- Message Structure:
CMAC_SecurityMode_Config_REQ
. (IntegerType)cellId = 0
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity = 0
. . (BitStringType)startValue[20] = "00000000000000000010"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = -
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CMAC_SecurityModeCfgReq
- BinaryMessage:
30 0e 02 01 00 30 09 0a 01 00 03 04 04 00 00 20

- No.: 1569
- Timestamp: 20:44:15:372_0
- RFN: 3978
- Chip: 10496
- Event: Receive
- PCO: CMAC
- Message: CMAC_SecurityMode_Config_CNF
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 2
- Message Structure:
CMAC_SecurityMode_Config_CNF
. (IntegerType)cellId = 0
- Constraint:
ca_CMAC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 00

- No.: 1570
- Timestamp: 20:44:15:374_0
- RFN: 3978
- Chip: 18176
- Event: Send
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_REQ
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 3
- Message Structure:
CRLC_SecurityMode_Config_REQ
. (IntegerType)cellId = -1
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity = 0
. . (BitStringType)startValue[20] = "00000000000000000010"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = -
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CRLC_SecurityModeCfgReq
- BinaryMessage:
30 0e 02 01 ff 30 09 0a 01 00 03 04 04 00 00 20

- No.: 1571
- Timestamp: 20:44:15:376_0
- RFN: 3978
- Chip: 24576
- Event: Receive
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_CNF
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 4
- Message Structure:
CRLC_SecurityMode_Config_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1592
- Timestamp: 20:44:15:405_0
- RFN: 3981
- Chip: 22016
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: pr_GenericSetupProcedures:lt_ReceiveResponseToPaging LINE 2
- Message Structure:
RRC_DataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. (START_Value)start[20] = '00000000000000000010'B
. SERVICEREQUEST
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)gMMProtocolDiscriminator[4] = '1000'B
. . (MsgType)msgType[8] = '00001100'B
. . ServiceType_v
. . . (B1)spare1[1] = '0'B
. . . (B3)type[3] = '010'B
. . CiphKeySeqNum
. . . (B1)spare1[1] = '0'B
. . . (KeySeq)keySeq[3] = '000'B
. . MS_Identity_lv
. . . (Length)iel[1] = '05'O
. . . (B4)iDigit1[4] = '1111'B
. . . (B1)oddEvenInd[1] = '0'B
. . . (B3)typeOfId[3] = '100'B
. . . (OctetStringType)otherDigits[4] = '12345678'O
. . PDP_ContextStatus
. . . (IEI8)iei[8] = '00110010'B
. . . (Length)iel[1] = '02'O
. . . (BitStringType)nSAPI[16] = '0000000000000000'B
- Constraint:
car_PS_InitDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 03 04 04 00 00 20 08 0c 20 05 f4 12 34 56 78 32 02 00 00

- No.: 1626
- Timestamp: 20:44:15:419_0
- RFN: 3982
- Chip: 36352
- Event: Send
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_REQ
- Source: ts_SS_DownloadSecurityKey:lt_DownloadKeyCRLC LINE 1
- Message Structure:
CRLC_SecurityMode_Config_REQ
. (IntegerType)cellId = -1
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity = 1
. . (BitStringType)startValue[20] = "00000000000000000010"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = '01010111010101100101000101010000010100110101001001011101010111000101111101011110010110010101100001011011010110100101010101010100'B
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CRLC_SecurityModeCfgReq
- BinaryMessage:
30 21 02 01 ff 30 1c 0a 01 01 03 04 04 00 00 20 03 11 00 57 56 51 50 53 52 5d 5c 5f 5e 59 58 5b 5a 55 54

- No.: 1627
- Timestamp: 20:44:15:421_0
- RFN: 3983
- Chip: 4864
- Event: Receive
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_CNF
- Source: ts_SS_DownloadSecurityKey:lt_DownloadKeyCRLC LINE 2
- Message Structure:
CRLC_SecurityMode_Config_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1634
- Timestamp: 20:44:15:424_0
- RFN: 3983
- Chip: 18944
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 1
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
. (IntegerType)count_I_LSB_UL = -
. (IntegerType)count_I_LSB_DL = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 00 02 01 00 02 01 00

- No.: 1635
- Timestamp: 20:44:15:426_0
- RFN: 3983
- Chip: 26112
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 2
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 00 02 01 00

- No.: 1636
- Timestamp: 20:44:15:428_0
- RFN: 3983
- Chip: 33280
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 3
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. (IntegerType)count_I_LSB_UL = -
. (IntegerType)count_I_LSB_DL = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 01 02 01 00

- No.: 1637
- Timestamp: 20:44:15:430_0
- RFN: 3984
- Chip: 2304
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 4
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 1638
- Timestamp: 20:44:15:432_0
- RFN: 3984
- Chip: 8960
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 5
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. (IntegerType)count_I_LSB_UL = -
. (IntegerType)count_I_LSB_DL = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 02 02 01 00

- No.: 1639
- Timestamp: 20:44:15:433_0
- RFN: 3984
- Chip: 16128
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 6
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 1640
- Timestamp: 20:44:15:435_0
- RFN: 3984
- Chip: 23552
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 7
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
. (IntegerType)count_I_LSB_UL = -
. (IntegerType)count_I_LSB_DL = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 03 02 01 00

- No.: 1641
- Timestamp: 20:44:15:437_0
- RFN: 3984
- Chip: 30720
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 8
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 1642
- Timestamp: 20:44:15:439_0
- RFN: 3984
- Chip: 37632
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 9
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
. (IntegerType)count_I_LSB_UL = -
. (IntegerType)count_I_LSB_DL = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 04 02 01 00

- No.: 1643
- Timestamp: 20:44:15:441_0
- RFN: 3985
- Chip: 6400
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 10
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 1647
- Timestamp: 20:44:15:444_0
- RFN: 3985
- Chip: 17920
- Event: Send
- PCO: CRLC
- Message: CRLC_Integrity_Activate_REQ
- Source: ts_CRLC_DL_Integrity LINE 1
- Message Structure:
CRLC_Integrity_Activate_REQ
. (IntegerType)cellId = -1
. (CN_DomainIdentity)cn_DomainIdentity = 1
. IntegrityActivationInfo
. . IntegrityProtectionModeInfo
. . . IntegrityProtectionModeCommand
. . . . startIntegrityProtection
. . . . . (BitStringType)integrityProtInitNumber[32] = "00000000000000000000000000000001"
. . . (IntegrityProtectionAlgorithm)integrityProtectionAlgorithm = 0
- Constraint:
ca_CRLC_DL_IntegrityActivateReq
- BinaryMessage:
30 15 02 01 ff 0a 01 01 30 0d 30 30 07 03 05 00 00 00 00 01 0a 01 00

- No.: 1648
- Timestamp: 20:44:15:446_0
- RFN: 3985
- Chip: 24320
- Event: Receive
- PCO: CRLC
- Message: CRLC_Integrity_Activate_CNF
- Source: ts_CRLC_DL_Integrity LINE 2
- Message Structure:
CRLC_Integrity_Activate_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_IntegrityActivateCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1655
- Timestamp: 20:44:15:449_0
- RFN: 3986
- Chip: 512
- Event: Send
- PCO: CRLC
- Message: CRLC_Integrity_Activate_REQ
- Source: ts_RB2_UL_IntegrityActivate LINE 1
- Message Structure:
CRLC_Integrity_Activate_REQ
. (IntegerType)cellId = -1
. (CN_DomainIdentity)cn_DomainIdentity = 1
. IntegrityActivationInfo
. . IntegrityProtActivationInfoList
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity = 2
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
- Constraint:
ca_CRLC_UL_IntegrityActivateReq
- BinaryMessage:
30 10 02 01 ff 0a 01 01 30 08 30 06 02 01 02 02 01 00

- No.: 1656
- Timestamp: 20:44:15:451_0
- RFN: 3986
- Chip: 6656
- Event: Receive
- PCO: CRLC
- Message: CRLC_Integrity_Activate_CNF
- Source: ts_RB2_UL_IntegrityActivate LINE 2
- Message Structure:
CRLC_Integrity_Activate_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_IntegrityActivateCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1662
- Timestamp: 20:44:15:457_0
- RFN: 3986
- Chip: 30464
- Event: Send
- PCO: AM
- Message: RLC_AM_DATA_REQ
- Source: ts_RRC_Security:lt_SendSecurityModeCommand LINE 7
- Message Structure:
RLC_AM_DATA_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. AmConfirmationRequest
. aM_message
. . DL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00000000000000000000000000000000"
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . DL_DCCH_MessageType
. . . . SecurityModeCommand
. . . . . r3
. . . . . . SecurityModeCommand_r3_IEs
. . . . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . . . SecurityCapability
. . . . . . . . (BitStringType)cipheringAlgorithmCap[16] = '0000000000000011'B
. . . . . . . . (BitStringType)integrityProtectionAlgorithmCap[16] = '0000000000000010'B
. . . . . . . CipheringModeInfo
. . . . . . . IntegrityProtectionModeInfo
. . . . . . . . IntegrityProtectionModeCommand
. . . . . . . . . startIntegrityProtection
. . . . . . . . . . (BitStringType)integrityProtInitNumber[32] = "00000000000000000000000000000001"
. . . . . . . . (IntegrityProtectionAlgorithm)integrityProtectionAlgorithm = 0
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity = 1
. . . . . . . InterRAT_UE_SecurityCapList
. . . . . . laterNonCriticalExtensions
- Constraint:
cas_RRC_SecModeCmd
- BinaryMessage:
30 17 02 01 ff 02 01 02 05 00 80 00 00 00 04 04 00 01 80 01 40 00 00 00 30

- No.: 1668
- Timestamp: 20:44:15:593_0
- RFN: 4000
- Chip: 11776
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_IND
- Source: ts_RRC_Security:lt_StartSecurity_UE LINE 8
- Message Structure:
RLC_AM_DATA_IND
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. IntegrityResult
. . (IntegrityStatus)integrityUsed = 0
. aM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "11101101011010000100111100101101"
. . . . (IntegerType)rrc_MessageSequenceNumber = 1
. . . UL_DCCH_MessageType
. . . . SecurityModeComplete
. . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . IntegrityProtActivationInfo
. . . . . . RRC_MessageSequenceNumberList
. . . . . . . (IntegerType)_elem = 0
. . . . . . . (IntegerType)_elem = 0
. . . . . . . (IntegerType)_elem = 0
. . . . . . . (IntegerType)_elem = 0
. . . . . . . (IntegerType)_elem = 0
. . . . . laterNonCriticalExtensions
. . . . . . (BitStringType)securityModeComplete_r3_add_ext = 0
. . . . . . nonCriticalExtensions
- Constraint:
car_RRC_SecModeCmpl
- BinaryMessage:
30 12 02 01 ff 02 01 02 0a 01 00 f6 b4 27 96 8d 21 00 00 00

- No.: 1669
- Timestamp: 20:44:15:594_0
- RFN: 4000
- Chip: 16128
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_Security:lt_StartSecurity_UE LINE 8
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1671
- Timestamp: 20:44:15:598_0
- RFN: 4000
- Chip: 32256
- Event: Send
- PCO: CRLC
- Message: CRLC_Integrity_Activate_REQ
- Source: ts_CRLC_UL_Integrity LINE 1
- Message Structure:
CRLC_Integrity_Activate_REQ
. (IntegerType)cellId = -1
. (CN_DomainIdentity)cn_DomainIdentity = 1
. IntegrityActivationInfo
. . IntegrityProtActivationInfoList
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity = 0
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity = 1
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity = 3
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity = 4
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
- Constraint:
ca_CRLC_UL_IntegrityActivateReq
- BinaryMessage:
30 28 02 01 ff 0a 01 01 30 20 30 06 02 01 00 02 01 00 30 06 02 01 01 02 01 00 30 06 02 01 03 02 01 00 30 06 02 01 04 02 01 00

- No.: 1672
- Timestamp: 20:44:15:600_0
- RFN: 4001
- Chip: 1024
- Event: Receive
- PCO: CRLC
- Message: CRLC_Integrity_Activate_CNF
- Source: ts_CRLC_UL_Integrity LINE 2
- Message Structure:
CRLC_Integrity_Activate_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_IntegrityActivateCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1684
- Timestamp: 20:44:15:624_0
- RFN: 4003
- Chip: 17664
- Event: Send
- PCO: Dc
- Message: RRC_DataReq
- Source: ts_TC_ActivateRB_TestMode LINE 7
- Message Structure:
RRC_DataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[-1] = -
. (SapId)sapId[1] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. ACTIVATERBTESTMODE
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)tCProtocolDiscriminator[4] = '1111'B
. . (MsgType)msgType[8] = '01000100'B
- Constraint:
ca_PS_DataReq
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 0f 44

- No.: 1685
- Timestamp: 20:44:15:625_0
- RFN: 4003
- Chip: 21504
- Event: Start Timer
- Source: ts_TC_ActivateRB_TestMode LINE 7
- Message Structure:
no details available
- Constraint:
t_Dly (5000 Ms)
- BinaryMessage:

- No.: 1689
- Timestamp: 20:44:15:750_0
- RFN: 4016
- Chip: 4352
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_TC_ActivateRB_TestMode LINE 8
- Message Structure:
RRC_DataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. (START_Value)start[0] = -
. ACTIVATERBTESTMODECOMPLETE
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)tCProtocolDiscriminator[4] = '1111'B
. . (MsgType)msgType[8] = '01000101'B
- Constraint:
car_PS_UplinkDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 0f 45

- No.: 1690
- Timestamp: 20:44:15:751_0
- RFN: 4016
- Chip: 7680
- Event: Cancel Timer
- Source: ts_TC_ActivateRB_TestMode LINE 8
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 1691
- Timestamp: 20:44:15:752_0
- RFN: 4016
- Chip: 8704
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_TC_ActivateRB_TestMode LINE 8
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1710
- Timestamp: 20:44:15:813_0
- RFN: 4022
- Chip: 13568
- Event: Send
- PCO: CPHY
- Message: CPHY_Frame_Number_REQ
- Source: ts_RRC_SetUpRAB_AM_7_RLC LINE 2
- Message Structure:
CPHY_Frame_Number_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
cas_GetFrameNum
- BinaryMessage:
30 06 02 01 00 02 01 1a

- No.: 1714
- Timestamp: 20:44:15:886_0
- RFN: 4029
- Chip: 25344
- Event: Receive
- PCO: CPHY
- Message: CPHY_Frame_Number_CNF
- Source: ts_RRC_SetUpRAB_AM_7_RLC LINE 3
- Message Structure:
CPHY_Frame_Number_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
. (IntegerType)frameNumber = 182
- Constraint:
car_GetFrameNum
- BinaryMessage:
30 0a 02 01 00 02 01 1a 02 02 00 b6

- No.: 1718
- Timestamp: 20:44:16:097_0
- RFN: 4050
- Chip: 30208
- Event: Send
- PCO: AM
- Message: RLC_AM_DATA_REQ
- Source: ts_RRC_SetUpRAB_AM_7_RLC:lt_SendRAB_SetupCS_OrPS LINE 4
- Message Structure:
RLC_AM_DATA_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. AmConfirmationRequest
. . (IntegerType)confirmationRequested = 0
. aM_message
. . DL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00000000000000000000000000000000"
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . DL_DCCH_MessageType
. . . . RadioBearerSetup
. . . . . r3
. . . . . . RadioBearerSetup_r3_IEs
. . . . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . . . IntegrityProtectionModeInfo
. . . . . . . CipheringModeInfo
. . . . . . . (IntegerType)activationTime = 168
. . . . . . . U_RNTI
. . . . . . . (BitStringType)new_C_RNTI[16] = -
. . . . . . . (RRC_StateIndicator)rrc_StateIndicator = 0
. . . . . . . (IntegerType)utran_DRX_CycleLengthCoeff = -
. . . . . . . (BitStringType)ura_Identity[0] = -
. . . . . . . CN_InformationInfo
. . . . . . . SRB_InformationSetupList
. . . . . . . RAB_InformationSetupList
. . . . . . . . RAB_InformationSetup
. . . . . . . . . RAB_Info
. . . . . . . . . . RAB_Identity
. . . . . . . . . . . (BitStringType)gsm_MAP_RAB_Identity[8] = '00000101'B
. . . . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = 1
. . . . . . . . . . (BitStringType)nas_Synchronisation_Indicator[0] = -
. . . . . . . . . . (Re_EstablishmentTimer)re_EstablishmentTimer = 0
. . . . . . . . . RB_InformationSetupList
. . . . . . . . . . RB_InformationSetup
. . . . . . . . . . . (IntegerType)rb_Identity = 20
. . . . . . . . . . . PDCP_Info
. . . . . . . . . . . RLC_InfoChoice
. . . . . . . . . . . . RLC_Info
. . . . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . . . MaxDAT_Retransmissions
. . . . . . . . . . . . . . . . . (MaxDAT)maxDAT = 3
. . . . . . . . . . . . . . . . . (TimerMRW)timerMRW = 13
. . . . . . . . . . . . . . . . . (MaxMRW)maxMRW = 1
. . . . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize = 1
. . . . . . . . . . . . . . . (TimerRST)timerRST = 9
. . . . . . . . . . . . . . . (MaxRST)max_RST = 1
. . . . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit = -
. . . . . . . . . . . . . . . . (TimerPoll)timerPoll = -
. . . . . . . . . . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . . . . . . . . . (Poll_SDU)poll_SDU = -
. . . . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . . . (PollWindow)pollWindow = -
. . . . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize = 1
. . . . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit = -
. . . . . . . . . . . . . . . . (TimerEPC)timerEPC = -
. . . . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = FALSE
. . . . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . . . . . . . . RB_MappingInfo
. . . . . . . . . . . . RB_MappingOption
. . . . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . . . (IntegerType)dch = 1
. . . . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 7
. . . . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 7
. . . . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . . . (IntegerType)dch = 6
. . . . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 7
. . . . . . . RB_InformationAffectedList
. . . . . . . DL_CounterSynchronisationInfo
. . . . . . . UL_CommonTransChInfo
. . . . . . . . TFC_Subset
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . TFCS
. . . . . . . . . . . ExplicitTFCS_Configuration
. . . . . . . . . . . . TFCS_ReconfAdd
. . . . . . . . . . . . . ctfcSize
. . . . . . . . . . . . . . ctfc4Bit
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . . . . . . . (IntegerType)ctfc4 = 0
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . . . . . . . (IntegerType)ctfc4 = 1
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . . . . . . . (IntegerType)ctfc4 = 2
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . . . . . . . (IntegerType)ctfc4 = 3
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 11
. . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . UL_DeletedTransChInfoList
. . . . . . . UL_AddReconfTransChInfoList
. . . . . . . . UL_AddReconfTransChInformation
. . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType = 0
. . . . . . . . . (IntegerType)transportChannelIdentity = 1
. . . . . . . . . TransportFormatSet
. . . . . . . . . . DedicatedTransChTFS
. . . . . . . . . . . tti
. . . . . . . . . . . . DedicatedDynamicTF_InfoList
. . . . . . . . . . . . . DedicatedDynamicTF_Info
. . . . . . . . . . . . . . rlc_Size
. . . . . . . . . . . . . . . OctetModeRLC_SizeInfoType1
. . . . . . . . . . . . . . . . (IntegerType)sizeType1 = 16
. . . . . . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . LogicalChannelList
. . . . . . . . . . . SemistaticTF_Information
. . . . . . . . . . . . ChannelCodingType
. . . . . . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . . . . . (IntegerType)rateMatchingAttribute = 155
. . . . . . . . . . . . (CRC_Size)crc_Size = 3
. . . . . . . . UL_AddReconfTransChInformation
. . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType = 0
. . . . . . . . . (IntegerType)transportChannelIdentity = 5
. . . . . . . . . TransportFormatSet
. . . . . . . . . . DedicatedTransChTFS
. . . . . . . . . . . tti
. . . . . . . . . . . . DedicatedDynamicTF_InfoList
. . . . . . . . . . . . . DedicatedDynamicTF_Info
. . . . . . . . . . . . . . rlc_Size
. . . . . . . . . . . . . . . BitModeRLC_SizeInfo
. . . . . . . . . . . . . . . . sizeType2
. . . . . . . . . . . . . . . . . (IntegerType)part1 = 2
. . . . . . . . . . . . . . . . . (IntegerType)part2 = -
. . . . . . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . LogicalChannelList
. . . . . . . . . . . SemistaticTF_Information
. . . . . . . . . . . . ChannelCodingType
. . . . . . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . . . . . (IntegerType)rateMatchingAttribute = 170
. . . . . . . . . . . . (CRC_Size)crc_Size = 3
. . . . . . . modeSpecificTransChInfo
. . . . . . . . fdd
. . . . . . . . . (IntegerType)cpch_SetID = -
. . . . . . . . . DRAC_StaticInformationList
. . . . . . . DL_CommonTransChInfo
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . dl_Parameters
. . . . . . . DL_DeletedTransChInfoList
. . . . . . . DL_AddReconfTransChInfoList
. . . . . . . . DL_AddReconfTransChInformation
. . . . . . . . . (DL_TrCH_Type)dl_TransportChannelType = 0
. . . . . . . . . (IntegerType)dl_transportChannelIdentity = 6
. . . . . . . . . tfs_SignallingMode
. . . . . . . . . . UL_TransportChannelIdentity
. . . . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType = 0
. . . . . . . . . . . (IntegerType)ul_TransportChannelIdentity = 1
. . . . . . . . . QualityTarget
. . . . . . . . . . (IntegerType)bler_QualityValue = -20
. . . . . . . . . TM_SignallingInfo
. . . . . . . . DL_AddReconfTransChInformation
. . . . . . . . . (DL_TrCH_Type)dl_TransportChannelType = 0
. . . . . . . . . (IntegerType)dl_transportChannelIdentity = 10
. . . . . . . . . tfs_SignallingMode
. . . . . . . . . . UL_TransportChannelIdentity
. . . . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType = 0
. . . . . . . . . . . (IntegerType)ul_TransportChannelIdentity = 5
. . . . . . . . . QualityTarget
. . . . . . . . . . (IntegerType)bler_QualityValue = -20
. . . . . . . . . TM_SignallingInfo
. . . . . . . FrequencyInfo
. . . . . . . (IntegerType)maxAllowedUL_TX_Power = 33
. . . . . . . UL_ChannelRequirement
. . . . . . . . UL_DPCH_Info
. . . . . . . . . UL_DPCH_PowerControlInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (IntegerType)dpcch_PowerOffset = -40
. . . . . . . . . . . (IntegerType)pc_Preamble = 1
. . . . . . . . . . . (IntegerType)sRB_delay = 7
. . . . . . . . . . . PowerControlAlgorithm
. . . . . . . . . . . . (IntegerType)algorithm1 = 1
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (ScramblingCodeType)scramblingCodeType = 1
. . . . . . . . . . . (IntegerType)scramblingCode = 0
. . . . . . . . . . . (IntegerType)numberOfDPDCH = -
. . . . . . . . . . . (SpreadingFactor)spreadingFactor = 4
. . . . . . . . . . . (BooleanType)tfci_Existence = TRUE
. . . . . . . . . . . (IntegerType)numberOfFBI_Bits = -
. . . . . . . . . . . (PuncturingLimit)puncturingLimit = 15
. . . . . . . modeSpecificPhysChInfo
. . . . . . . . fdd
. . . . . . . . . DL_PDSCH_Information
. . . . . . . DL_CommonInformation
. . . . . . . . DL_DPCH_InfoCommon
. . . . . . . . . cfnHandling
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . DL_DPCH_PowerControlInfo
. . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . (DPC_Mode)dpc_Mode = 0
. . . . . . . . . . . (IntegerType)powerOffsetPilot_pdpdch = 0
. . . . . . . . . . . Dl_rate_matching_restriction
. . . . . . . . . . . SF512_AndPilot
. . . . . . . . . . . . (PilotBits128)sfd128 = 0
. . . . . . . . . . . (PositionFixedOrFlexible)positionFixedOrFlexible = 1
. . . . . . . . . . . (BooleanType)tfci_Existence = TRUE
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . (IntegerType)defaultDPCH_OffsetValue = -
. . . . . . . . . . DPCH_CompressedModeInfo
. . . . . . . . . . (TX_DiversityMode)tx_DiversityMode = 0
. . . . . . . . . . SSDT_Information
. . . . . . . DL_InformationPerRL_List
. . . . . . . . DL_InformationPerRL
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . PrimaryCPICH_Info
. . . . . . . . . . . . (IntegerType)primaryScramblingCode = 100
. . . . . . . . . . . PDSCH_SHO_DCH_Info
. . . . . . . . . . . PDSCH_CodeMapping
. . . . . . . . . DL_DPCH_InfoPerRL
. . . . . . . . . . fdd
. . . . . . . . . . . (PCPICH_UsageForChannelEst)pCPICH_UsageForChannelEst = 0
. . . . . . . . . . . (IntegerType)dpch_FrameOffset = 0
. . . . . . . . . . . SecondaryCPICH_Info
. . . . . . . . . . . DL_ChannelisationCodeList
. . . . . . . . . . . . DL_ChannelisationCode
. . . . . . . . . . . . . (IntegerType)secondaryScramblingCode = 1
. . . . . . . . . . . . . SF512_AndCodeNumber
. . . . . . . . . . . . . . (IntegerType)sf128 = 0
. . . . . . . . . . . . . (ScramblingCodeChange)scramblingCodeChange = -
. . . . . . . . . . . (IntegerType)tpc_CombinationIndex = 0
. . . . . . . . . . . (SSDT_CellIdentity)ssdt_CellIdentity = -
. . . . . . . . . . . (ClosedLoopTimingAdjMode)closedLoopTimingAdjMode = -
. . . . . . . . . SCCPCH_InfoForFACH
. . . . . . v3a0NonCriticalExtensions
. . . . . . . RadioBearerSetup_v3a0ext
. . . . . . . . (BitStringType)new_DSCH_RNTI[16] = -
. . . . . . . laterNonCriticalExtensions
- Constraint:
cas_RB_SetUpAM_WithCnf
- BinaryMessage:
30 4f 02 01 ff 02 01 02 02 01 00 80 00 00 00 03 92 04 ba f2 a0 00 16 09 b3 1e 91 92 06 44 06 80 67 21 58 81 00 e0 91 49 24 ca fc 08 02 09 00 88 e6 98 84 02 20 88 ea 58 30 c2 c0 ae 26 25 74 d2 a3 d1 00 00 00 9f 24 02 b1 02 06 40 00 08 28 00 00

- No.: 1723
- Timestamp: 20:44:16:277_0
- RFN: 4068
- Chip: 28672
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_CNF
- Source: ts_RRC_SetUpRAB_AM_7_RLC LINE 6
- Message Structure:
RLC_AM_DATA_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. (IntegerType)mui = 0
- Constraint:
car_AM_DataMuiCnf
- BinaryMessage:
30 09 02 01 ff 02 01 02 02 01 00

- No.: 1730
- Timestamp: 20:44:16:423_0
- RFN: 4083
- Chip: 15616
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Modify_REQ
- Source: ts_SS_2DCH_Modify LINE 3
- Message Structure:
CPHY_RL_Modify_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
. (RatType)ratType = 0
. CphyRlModifyReq
. . SS_ActivationTime
. . . (IntegerType)activationCFN = 168
. . physicalChannelInfo
. . . DPCHInfo
. . . . UL_DPCH_Info
. . . . DL_DPCHInfo
. . . . . DL_CommonInformation
. . . . . . DL_DPCH_InfoCommon
. . . . . . . cfnHandling
. . . . . . . modeSpecificInfo
. . . . . . . . fdd
. . . . . . . . . DL_DPCH_PowerControlInfo
. . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . fdd
. . . . . . . . . . . . (DPC_Mode)dpc_Mode = 0
. . . . . . . . . (IntegerType)powerOffsetPilot_pdpdch = 0
. . . . . . . . . Dl_rate_matching_restriction
. . . . . . . . . SF512_AndPilot
. . . . . . . . . . (PilotBits128)sfd128 = 0
. . . . . . . . . (PositionFixedOrFlexible)positionFixedOrFlexible = 1
. . . . . . . . . (BooleanType)tfci_Existence = TRUE
. . . . . . modeSpecificInfo
. . . . . . . fdd
. . . . . . . . (IntegerType)defaultDPCH_OffsetValue = -
. . . . . . . . DPCH_CompressedModeInfo
. . . . . . . . (TX_DiversityMode)tx_DiversityMode = 0
. . . . . . . . SSDT_Information
. . . . . DL_DPCH_InfoPerRL
. . . . . . fdd
. . . . . . . (PCPICH_UsageForChannelEst)pCPICH_UsageForChannelEst = 0
. . . . . . . (IntegerType)dpch_FrameOffset = 0
. . . . . . . SecondaryCPICH_Info
. . . . . . . DL_ChannelisationCodeList
. . . . . . . . DL_ChannelisationCode
. . . . . . . . . (IntegerType)secondaryScramblingCode = 1
. . . . . . . . . SF512_AndCodeNumber
. . . . . . . . . . (IntegerType)sf128 = 0
. . . . . . . . . (ScramblingCodeChange)scramblingCodeChange = -
. . . . . . . (IntegerType)tpc_CombinationIndex = 0
. . . . . . . (SSDT_CellIdentity)ssdt_CellIdentity = -
. . . . . . . (ClosedLoopTimingAdjMode)closedLoopTimingAdjMode = -
. . . . . (IntegerType)powerOffsetOfTFCI_PO1 = 0
. . . . . (IntegerType)powerOffsetOfTPC_PO2 = 0
. . . . . (IntegerType)powerOffsetOfPILOT_PO3 = 0
. . . . . (IntegerType)dl_TxPower = -5
. . . . . (IntegerType)dl_TxPowerMax = 15
. . . . . (IntegerType)dl_TxPowerMin = -35
- Constraint:
ca_DL_DPCH_ModifyInfo
- BinaryMessage:
30 5e 02 01 00 02 01 1a 0a 01 00 30 53 02 02 00 a8 30 4d 30 4b 30 21 30 19 05 00 30 30 14 30 06 30 30 03 0a 01 00 02 01 00 0a 01 00 0a 01 01 01 01 ff 30 30 03 0a 01 00 30 30 13 0a 01 00 02 01 00 30 08 30 06 02 01 01 02 01 00 02 01 00 02 01 00 02 01 00 02 01 00 02 01 fb 02 01 0f 02 01 dd

- No.: 1734
- Timestamp: 20:44:16:474_0
- RFN: 4088
- Chip: 15104
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Modify_CNF
- Source: ts_SS_2DCH_Modify LINE 4
- Message Structure:
CPHY_RL_Modify_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
ca_RL_ModifyCnf
- BinaryMessage:
30 06 02 01 00 02 01 1a

- No.: 1735
- Timestamp: 20:44:16:501_0
- RFN: 4091
- Chip: 3584
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Config_REQ
- Source: ts_SS_2DCH_Modify LINE 5
- Message Structure:
CPHY_TrCH_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
. (RatType)ratType = 0
. CphyTrchConfigReq
. . SS_ActivationTime
. . . (IntegerType)activationCFN = 168
. . ulconnectedTrCHList
. . TFCS
. . dlconnectedTrCHList
. . . CphyTrchConfigReq_setseq_1
. . . . (IntegerType)trchid = 6
. . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 144
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional = 1
. . . . . . (IntegerType)rateMatchingAttribute = 155
. . . . . . (CRC_Size)crc_Size = 3
. . . CphyTrchConfigReq_setseq_1
. . . . (IntegerType)trchid = 10
. . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 148
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional = 1
. . . . . . (IntegerType)rateMatchingAttribute = 170
. . . . . . (CRC_Size)crc_Size = 3
. . TFCS
. . . ExplicitTFCS_Configuration
. . . . TFCS_ReconfAdd
. . . . . ctfcSize
. . . . . . ctfc4Bit
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 0
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 1
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 2
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 3
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . fdd
. . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 9
. . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
- Constraint:
ca_TrChCfgInfo
- BinaryMessage:
30 81 96 02 01 00 02 01 1a 0a 01 00 30 81 8a 02 02 00 a8 30 4c 30 24 02 01 06 0a 01 00 30 1c 30 0e 30 0c 02 02 00 90 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 9b 0a 01 03 30 24 02 01 0a 0a 01 00 30 1c 30 0e 30 0c 02 02 00 94 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 aa 0a 01 03 30 36 30 30 33 30 08 02 01 00 30 03 02 01 00 30 08 02 01 01 30 03 02 01 00 30 08 02 01 02 30 03 02 01 00 30 13 02 01 03 30 0e 30 0c 30 30 03 02 01 09 02 01 0f 02 01 00

- No.: 1739
- Timestamp: 20:44:16:550_0
- RFN: 4096
- Chip: 1024
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Config_CNF
- Source: ts_SS_2DCH_Modify LINE 6
- Message Structure:
CPHY_TrCH_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
ca_TrChCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 1a

- No.: 1740
- Timestamp: 20:44:16:609_0
- RFN: 4101
- Chip: 34816
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_SS_2DCH_Modify LINE 7
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
. (RatType)ratType = 0
. configMessage
. . CmacConfigReq
. . . SS_ActivationTime
. . . . (IntegerType)activationCFN = 168
. . . UE_Info
. . . . U_RNTI
. . . . (BitStringType)c_RNTI[16] = -
. . . TrCHInfo
. . . . ulconnectedTrCHList
. . . . TFCS
. . . . dlconnectedTrCHList
. . . . . TrCHInfo_setseq_1
. . . . . . (IntegerType)trchid = 6
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 144
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . (IntegerType)rateMatchingAttribute = 155
. . . . . . . . (CRC_Size)crc_Size = 3
. . . . . TrCHInfo_setseq_1
. . . . . . (IntegerType)trchid = 10
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 148
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . (IntegerType)rateMatchingAttribute = 170
. . . . . . . . (CRC_Size)crc_Size = 3
. . . . TFCS
. . . . . ExplicitTFCS_Configuration
. . . . . . TFCS_ReconfAdd
. . . . . . . ctfcSize
. . . . . . . . ctfc4Bit
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 0
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 1
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 2
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 3
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 9
. . . . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . TrCH_LogCHMappingList1
. . . . ulconnectedTrCHList
. . . . dlconnectedTrCHList
. . . . . TrCH_LogCHMappingList1_setseq_1
. . . . . . (IntegerType)trchid = 6
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 7
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 5
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 7
. . . . . . . . (IntegerType)rB_Identity = -12
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . TrCH_LogCHMappingList1_setseq_1
. . . . . . (IntegerType)trchid = 10
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 1
. . . . . . . . (IntegerType)rB_Identity = 1
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 2
. . . . . . . . (IntegerType)rB_Identity = 2
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 3
. . . . . . . . (IntegerType)rB_Identity = 3
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 4
. . . . . . . . (IntegerType)rB_Identity = 4
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_CMAC_ReconfigInfo
- BinaryMessage:
30 82 01 22 02 01 ff 02 01 1a 0a 01 00 30 82 01 15 02 02 00 a8 30 00 30 81 80 30 46 30 21 02 01 06 30 1c 30 0e 30 0c 02 02 00 90 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 9b 0a 01 03 30 21 02 01 0a 30 1c 30 0e 30 0c 02 02 00 94 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 aa 0a 01 03 30 36 30 30 33 30 08 02 01 00 30 03 02 01 00 30 08 02 01 01 30 03 02 01 00 30 08 02 01 02 30 03 02 01 00 30 13 02 01 03 30 0e 30 0c 30 30 03 02 01 09 02 01 0f 02 01 00 30 81 89 30 81 86 30 1d 02 01 06 30 18 30 16 30 11 0a 01 00 0a 01 00 02 01 07 0a 01 05 05 00 02 01 07 02 01 f4 30 65 02 01 0a 30 60 30 16 30 11 0a 01 00 0a 01 00 02 01 01 0a 01 04 05 00 02 01 01 02 01 01 30 16 30 11 0a 01 00 0a 01 00 02 01 02 0a 01 04 05 00 02 01 02 02 01 02 30 16 30 11 0a 01 00 0a 01 00 02 01 03 0a 01 04 05 00 02 01 03 02 01 03 30 16 30 11 0a 01 00 0a 01 00 02 01 04 0a 01 04 05 00 02 01 04 02 01 04

- No.: 1744
- Timestamp: 20:44:16:671_0
- RFN: 4108
- Chip: 6400
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_SS_2DCH_Modify LINE 8
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 1a

- No.: 1745
- Timestamp: 20:44:16:701_0
- RFN: 4111
- Chip: 6656
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Modify_REQ
- Source: ts_SS_2DCH_Modify LINE 9
- Message Structure:
CPHY_RL_Modify_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
. (RatType)ratType = 0
. CphyRlModifyReq
. . SS_ActivationTime
. . . (IntegerType)activationCFN = 168
. . physicalChannelInfo
. . . DPCHInfo
. . . . UL_DPCH_Info
. . . . . UL_DPCH_PowerControlInfo
. . . . . . fdd
. . . . . . . (IntegerType)dpcch_PowerOffset = -40
. . . . . . . (IntegerType)pc_Preamble = 1
. . . . . . . (IntegerType)sRB_delay = 7
. . . . . . . PowerControlAlgorithm
. . . . . . . . (IntegerType)algorithm1 = 1
. . . . . modeSpecificInfo
. . . . . . fdd
. . . . . . . (ScramblingCodeType)scramblingCodeType = 1
. . . . . . . (IntegerType)scramblingCode = 0
. . . . . . . (IntegerType)numberOfDPDCH = -
. . . . . . . (SpreadingFactor)spreadingFactor = 4
. . . . . . . (BooleanType)tfci_Existence = TRUE
. . . . . . . (IntegerType)numberOfFBI_Bits = -
. . . . . . . (PuncturingLimit)puncturingLimit = 15
. . . . DL_DPCHInfo
- Constraint:
ca_UL_DPCH_ModifyInfo
- BinaryMessage:
30 34 02 01 00 02 01 14 0a 01 00 30 29 02 02 00 a8 30 23 30 21 30 30 0c 02 01 d8 02 01 01 02 01 07 02 01 01 30 30 0f 0a 01 01 02 01 00 0a 01 04 01 01 ff 0a 01 0f

- No.: 1749
- Timestamp: 20:44:16:756_0
- RFN: 4116
- Chip: 26880
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Modify_CNF
- Source: ts_SS_2DCH_Modify LINE 10
- Message Structure:
CPHY_RL_Modify_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_RL_ModifyCnf
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 1750
- Timestamp: 20:44:16:788_0
- RFN: 4119
- Chip: 29696
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Config_REQ
- Source: ts_SS_2DCH_Modify LINE 11
- Message Structure:
CPHY_TrCH_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
. (RatType)ratType = 0
. CphyTrchConfigReq
. . SS_ActivationTime
. . . (IntegerType)activationCFN = 168
. . ulconnectedTrCHList
. . . CphyTrchConfigReq_setseq_0
. . . . (IntegerType)trchid = 1
. . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 144
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional = 1
. . . . . . (IntegerType)rateMatchingAttribute = 155
. . . . . . (CRC_Size)crc_Size = 3
. . . CphyTrchConfigReq_setseq_0
. . . . (IntegerType)trchid = 5
. . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 148
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional = 1
. . . . . . (IntegerType)rateMatchingAttribute = 170
. . . . . . (CRC_Size)crc_Size = 3
. . TFCS
. . . ExplicitTFCS_Configuration
. . . . TFCS_ReconfAdd
. . . . . ctfcSize
. . . . . . ctfc4Bit
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 0
. . . . . . . . PowerOffsetInformation
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 1
. . . . . . . . PowerOffsetInformation
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 2
. . . . . . . . PowerOffsetInformation
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 3
. . . . . . . . PowerOffsetInformation
. . dlconnectedTrCHList
. . TFCS
- Constraint:
ca_TrChCfgInfo
- BinaryMessage:
30 76 02 01 00 02 01 14 0a 01 00 30 6b 02 02 00 a8 30 4c 30 24 02 01 01 0a 01 00 30 1c 30 0e 30 0c 02 02 00 90 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 9b 0a 01 03 30 24 02 01 05 0a 01 00 30 1c 30 0e 30 0c 02 02 00 94 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 aa 0a 01 03 30 17 30 30 14 30 03 02 01 00 30 03 02 01 01 30 03 02 01 02 30 03 02 01 03

- No.: 1754
- Timestamp: 20:44:16:837_0
- RFN: 4124
- Chip: 29440
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Config_CNF
- Source: ts_SS_2DCH_Modify LINE 12
- Message Structure:
CPHY_TrCH_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_TrChCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 1755
- Timestamp: 20:44:16:897_0
- RFN: 4130
- Chip: 29440
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_SS_2DCH_Modify LINE 13
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
. (RatType)ratType = 0
. configMessage
. . CmacConfigReq
. . . SS_ActivationTime
. . . . (IntegerType)activationCFN = 168
. . . UE_Info
. . . . U_RNTI
. . . . (BitStringType)c_RNTI[16] = -
. . . TrCHInfo
. . . . ulconnectedTrCHList
. . . . . TrCHInfo_setseq_0
. . . . . . (IntegerType)trchid = 1
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 144
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . (IntegerType)rateMatchingAttribute = 155
. . . . . . . . (CRC_Size)crc_Size = 3
. . . . . TrCHInfo_setseq_0
. . . . . . (IntegerType)trchid = 5
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 148
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . (IntegerType)rateMatchingAttribute = 170
. . . . . . . . (CRC_Size)crc_Size = 3
. . . . TFCS
. . . . . ExplicitTFCS_Configuration
. . . . . . TFCS_ReconfAdd
. . . . . . . ctfcSize
. . . . . . . . ctfc4Bit
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 0
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 1
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 2
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 3
. . . . . . . . . . PowerOffsetInformation
. . . . dlconnectedTrCHList
. . . . TFCS
. . . TrCH_LogCHMappingList1
. . . . ulconnectedTrCHList
. . . . . TrCH_LogCHMappingList1_setseq_0
. . . . . . (IntegerType)trchid = 1
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 7
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 5
. . . . . . . . (IntegerType)rB_Identity = -12
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . TrCH_LogCHMappingList1_setseq_0
. . . . . . (IntegerType)trchid = 5
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . (IntegerType)rB_Identity = 1
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . (IntegerType)rB_Identity = 2
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . (IntegerType)rB_Identity = 3
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . (IntegerType)rB_Identity = 4
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . dlconnectedTrCHList
- Constraint:
ca_CMAC_ReconfigInfo
- BinaryMessage:
30 81 e6 02 01 ff 02 01 14 0a 01 00 30 81 da 02 02 00 a8 30 00 30 61 30 46 30 21 02 01 01 30 1c 30 0e 30 0c 02 02 00 90 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 9b 0a 01 03 30 21 02 01 05 30 1c 30 0e 30 0c 02 02 00 94 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 aa 0a 01 03 30 17 30 30 14 30 03 02 01 00 30 03 02 01 01 30 03 02 01 02 30 03 02 01 03 30 6f 30 6d 30 18 02 01 01 30 13 30 11 30 0c 0a 01 00 0a 01 00 02 01 07 0a 01 05 02 01 f4 30 51 02 01 05 30 4c 30 11 30 0c 0a 01 00 0a 01 00 02 01 01 0a 01 04 02 01 01 30 11 30 0c 0a 01 00 0a 01 00 02 01 02 0a 01 04 02 01 02 30 11 30 0c 0a 01 00 0a 01 00 02 01 03 0a 01 04 02 01 03 30 11 30 0c 0a 01 00 0a 01 00 02 01 04 0a 01 04 02 01 04

- No.: 1756
- Timestamp: 20:44:16:931_0
- RFN: 4134
- Chip: 5376
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_SS_2DCH_Modify LINE 14
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 14

- No.: 1759
- Timestamp: 20:44:16:942_0
- RFN: 4135
- Chip: 9984
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB_TM_Cfg_RLC LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = -12
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_TM_RLC_Mode
. . . . . . (BooleanType)segmentationIndication = TRUE
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 144
. . . . . UL_RLC_Mode
. . . . . . UL_TM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . (BooleanType)segmentationIndication = TRUE
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = 7
. . . . (IntegerType)dLlogicalChannelIdentity = 7
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_TM_Info
- BinaryMessage:
30 25 02 01 ff 02 01 f4 0a 01 00 30 1a 30 10 30 03 01 01 ff 30 09 02 02 00 90 30 03 01 01 ff 30 06 02 01 07 02 01 07

- No.: 1763
- Timestamp: 20:44:16:959_0
- RFN: 4136
- Chip: 36608
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB_TM_Cfg_RLC LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = -12
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 f4

- No.: 1771
- Timestamp: 20:44:16:981_0
- RFN: 4139
- Chip: 5888
- Event: Start Timer
- Source: ts_RRC_ReceiveRB_SetupCmpl LINE 2
- Message Structure:
no details available
- Constraint:
t_WaitMS (13500 Ms)
- BinaryMessage:

- No.: 1780
- Timestamp: 20:44:18:346_0
- RFN: 4275
- Chip: 23296
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_IND
- Source: ts_RRC_ReceiveRB_SetupCmpl:lt_CipheringNotStartedAM_RAB LINE 4
- Message Structure:
RLC_AM_DATA_IND
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. IntegrityResult
. . (IntegrityStatus)integrityUsed = 0
. aM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "01100111110100110110111001101110"
. . . . (IntegerType)rrc_MessageSequenceNumber = 2
. . . UL_DCCH_MessageType
. . . . RadioBearerSetupComplete
. . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . IntegrityProtActivationInfo
. . . . . (IntegerType)ul_TimingAdvance = 0
. . . . . (BitStringType)start_Value[20] = "00000000000000000100"
. . . . . (IntegerType)count_C_ActivationTime = 0
. . . . . UL_CounterSynchronisationInfo
. . . . . laterNonCriticalExtensions
. . . . . . (BitStringType)radioBearerSetupComplete_r3_add_ext = 0
. . . . . . nonCriticalExtensions
- Constraint:
car_RB_SetUpCmpl
- BinaryMessage:
30 12 02 01 ff 02 01 02 0a 01 00 b3 e9 b7 37 13 c8 00 00 08

- No.: 1781
- Timestamp: 20:44:18:347_0
- RFN: 4275
- Chip: 28672
- Event: Cancel Timer
- Source: ts_RRC_ReceiveRB_SetupCmpl:lt_CipheringNotStartedAM_RAB LINE 4
- Message Structure:
no details available
- Constraint:
t_WaitMS
- BinaryMessage:

- No.: 1782
- Timestamp: 20:44:18:348_0
- RFN: 4275
- Chip: 29696
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ReceiveRB_SetupCmpl:lt_CipheringNotStartedAM_RAB LINE 4
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1807
- Timestamp: 20:44:18:397_0
- RFN: 4280
- Chip: 28160
- Event: Send
- PCO: Dc
- Message: RRC_DataReq
- Source: ts_TC_CloseUE_TestLoop LINE 6
- Message Structure:
RRC_DataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[-1] = -
. (SapId)sapId[1] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. CLOSEUETESTLOOP
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)tCProtocolDiscriminator[4] = '1111'B
. . (MsgType)msgType[8] = '01000000'B
. . (UE_TestLoopMode)uE_TestLoopMode[1] = '00'O
. . UE_TestLoopMode1LB_Setup
. . . (Length)iel[1] = '03'O
. . . LB_SetupRB_IE
. . . . (BitStringType)rLC_SDU_Size[16] = '0000000001111000'B
. . . . (BitStringType)spare_2[3] = '000'B
. . . . (BitStringType)rB_Identity[5] = '10100'B
. . . LB_SetupRB_IE
. . . LB_SetupRB_IE
. . . LB_SetupRB_IE
- Constraint:
ca_PS_DataReq
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 0f 40 00 03 00 78 14

- No.: 1808
- Timestamp: 20:44:18:399_0
- RFN: 4280
- Chip: 33536
- Event: Start Timer
- Source: ts_TC_CloseUE_TestLoop LINE 6
- Message Structure:
no details available
- Constraint:
t_Dly (5000 Ms)
- BinaryMessage:

- No.: 1812
- Timestamp: 20:44:18:693_0
- RFN: 4310
- Chip: 12544
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_TC_CloseUE_TestLoop LINE 7
- Message Structure:
RRC_DataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. (START_Value)start[0] = -
. CLOSEUETESTLOOPCOMPLETE
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)tCProtocolDiscriminator[4] = '1111'B
. . (MsgType)msgType[8] = '01000001'B
- Constraint:
car_PS_UplinkDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 0f 41

- No.: 1813
- Timestamp: 20:44:18:694_0
- RFN: 4310
- Chip: 15872
- Event: Cancel Timer
- Source: ts_TC_CloseUE_TestLoop LINE 7
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 1814
- Timestamp: 20:44:18:694_1
- RFN: 4310
- Chip: 16640
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_TC_CloseUE_TestLoop LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1827
- Timestamp: 20:44:18:721_1
- RFN: 4313
- Chip: 6400
- Event: Start Timer
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 6
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 1834
- Timestamp: 20:44:18:734_0
- RFN: 4314
- Chip: 15104
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 1858
- Timestamp: 20:44:18:804_0
- RFN: 4321
- Chip: 17408
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000000'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'FFE665A5C5CA3452085408ABEECE4B'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 01 1e ff e6 65 a5 c5 ca 34 52 08 54 08 ab ee ce 4b

- No.: 1867
- Timestamp: 20:44:18:817_1
- RFN: 4322
- Chip: 29952
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 1868
- Timestamp: 20:44:18:818_0
- RFN: 4322
- Chip: 30976
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1873
- Timestamp: 20:44:18:834_0
- RFN: 4324
- Chip: 16384
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 1897
- Timestamp: 20:44:18:878_0
- RFN: 4328
- Chip: 35072
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000001'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '0B813FD337873F2CD1E29AE91BD6C8'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 09 1e 0b 81 3f d3 37 87 3f 2c d1 e2 9a e9 1b d6 c8

- No.: 1906
- Timestamp: 20:44:18:891_1
- RFN: 4330
- Chip: 8192
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 1907
- Timestamp: 20:44:18:892_0
- RFN: 4330
- Chip: 9216
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1912
- Timestamp: 20:44:18:908_0
- RFN: 4331
- Chip: 33024
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 1936
- Timestamp: 20:44:18:955_0
- RFN: 4336
- Chip: 22272
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000010'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'E14FDE630F8195688EBE465F09816A'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 11 1e e1 4f de 63 0f 81 95 68 8e be 46 5f 09 81 6a

- No.: 1945
- Timestamp: 20:44:18:969_1
- RFN: 4337
- Chip: 35584
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 1946
- Timestamp: 20:44:18:970_0
- RFN: 4337
- Chip: 36608
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1949
- Timestamp: 20:44:18:977_0
- RFN: 4338
- Chip: 25344
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000000'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = 'FFE665A5C5CA3452085408ABEECE4B'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 05 1e ff e6 65 a5 c5 ca 34 52 08 54 08 ab ee ce 4b

- No.: 1966
- Timestamp: 20:44:19:003_1
- RFN: 4341
- Chip: 11520
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1969
- Timestamp: 20:44:19:006_1
- RFN: 4341
- Chip: 24832
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 1993
- Timestamp: 20:44:19:054_0
- RFN: 4346
- Chip: 16384
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000011'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '8EEB1B83953DD362DAE3B06D5B76D8'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 19 1e 8e eb 1b 83 95 3d d3 62 da e3 b0 6d 5b 76 d8

- No.: 2002
- Timestamp: 20:44:19:067_1
- RFN: 4347
- Chip: 28672
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 2003
- Timestamp: 20:44:19:067_2
- RFN: 4347
- Chip: 29440
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2006
- Timestamp: 20:44:19:074_0
- RFN: 4348
- Chip: 18176
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000001'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '0B813FD337873F2CD1E29AE91BD6C8'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 0d 1e 0b 81 3f d3 37 87 3f 2c d1 e2 9a e9 1b d6 c8

- No.: 2023
- Timestamp: 20:44:19:100_2
- RFN: 4351
- Chip: 1792
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2026
- Timestamp: 20:44:19:103_1
- RFN: 4351
- Chip: 14592
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 2050
- Timestamp: 20:44:19:151_0
- RFN: 4356
- Chip: 4864
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000100'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'E3E53087EA645A09017FD99C3CACBB'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 21 1e e3 e5 30 87 ea 64 5a 09 01 7f d9 9c 3c ac bb

- No.: 2059
- Timestamp: 20:44:19:164_1
- RFN: 4357
- Chip: 18944
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 2060
- Timestamp: 20:44:19:165_0
- RFN: 4357
- Chip: 19712
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2063
- Timestamp: 20:44:19:172_0
- RFN: 4358
- Chip: 8704
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000010'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = 'E14FDE630F8195688EBE465F09816A'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 15 1e e1 4f de 63 0f 81 95 68 8e be 46 5f 09 81 6a

- No.: 2080
- Timestamp: 20:44:19:197_3
- RFN: 4360
- Chip: 30720
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2083
- Timestamp: 20:44:19:201_0
- RFN: 4361
- Chip: 5120
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 2107
- Timestamp: 20:44:19:249_0
- RFN: 4365
- Chip: 38144
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000101'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '46DF1CD61DA9C435F89943DF9CC34A'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 29 1e 46 df 1c d6 1d a9 c4 35 f8 99 43 df 9c c3 4a

- No.: 2116
- Timestamp: 20:44:19:262_1
- RFN: 4367
- Chip: 12288
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 2117
- Timestamp: 20:44:19:263_0
- RFN: 4367
- Chip: 13312
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2120
- Timestamp: 20:44:19:271_0
- RFN: 4368
- Chip: 2560
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000011'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '8EEB1B83953DD362DAE3B06D5B76D8'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 1d 1e 8e eb 1b 83 95 3d d3 62 da e3 b0 6d 5b 76 d8

- No.: 2137
- Timestamp: 20:44:19:297_0
- RFN: 4370
- Chip: 25344
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2140
- Timestamp: 20:44:19:300_1
- RFN: 4371
- Chip: 512
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 2164
- Timestamp: 20:44:19:348_0
- RFN: 4375
- Chip: 30976
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000110'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'DEE31AD6E24FA1903D53778D949742'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 31 1e de e3 1a d6 e2 4f a1 90 3d 53 77 8d 94 97 42

- No.: 2173
- Timestamp: 20:44:19:361_1
- RFN: 4377
- Chip: 5120
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 2174
- Timestamp: 20:44:19:361_2
- RFN: 4377
- Chip: 5888
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2177
- Timestamp: 20:44:19:369_0
- RFN: 4377
- Chip: 33792
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000100'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = 'E3E53087EA645A09017FD99C3CACBB'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 25 1e e3 e5 30 87 ea 64 5a 09 01 7f d9 9c 3c ac bb

- No.: 2194
- Timestamp: 20:44:19:394_3
- RFN: 4380
- Chip: 17664
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2197
- Timestamp: 20:44:19:398_0
- RFN: 4380
- Chip: 31232
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 2222
- Timestamp: 20:44:19:448_0
- RFN: 4385
- Chip: 34304
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000111'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '750DD49DE9CE9E430AD448A14575D8'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 3d 1e 75 0d d4 9d e9 ce 9e 43 0a d4 48 a1 45 75 d8

- No.: 2231
- Timestamp: 20:44:19:462_0
- RFN: 4387
- Chip: 8192
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 2232
- Timestamp: 20:44:19:462_1
- RFN: 4387
- Chip: 9216
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2235
- Timestamp: 20:44:19:469_0
- RFN: 4387
- Chip: 36864
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000101'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '46DF1CD61DA9C435F89943DF9CC34A'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 2d 1e 46 df 1c d6 1d a9 c4 35 f8 99 43 df 9c c3 4a

- No.: 2252
- Timestamp: 20:44:19:496_2
- RFN: 4390
- Chip: 26112
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2255
- Timestamp: 20:44:19:503_0
- RFN: 4391
- Chip: 15616
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000110'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = 'DEE31AD6E24FA1903D53778D949742'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 35 1e de e3 1a d6 e2 4f a1 90 3d 53 77 8d 94 97 42

- No.: 2272
- Timestamp: 20:44:19:529_2
- RFN: 4393
- Chip: 37376
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2275
- Timestamp: 20:44:19:533_0
- RFN: 4394
- Chip: 13056
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 2284
- Timestamp: 20:44:19:550_1
- RFN: 4396
- Chip: 3840
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 14
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 2285
- Timestamp: 20:44:19:550_2
- RFN: 4396
- Chip: 4864
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2290
- Timestamp: 20:44:19:568_1
- RFN: 4397
- Chip: 33792
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 2299
- Timestamp: 20:44:19:589_0
- RFN: 4399
- Chip: 32768
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 14
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 2300
- Timestamp: 20:44:19:589_1
- RFN: 4399
- Chip: 33536
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2303
- Timestamp: 20:44:19:605_0
- RFN: 4401
- Chip: 19712
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 5
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. STATUS_PDU
. . (DC_Field)dC_Field[1] = '0'B
. . (CtrlPDU_Type)type[3] = '000'B
. . SuperFields
. . (HexStringType)superFieldsAndPadRx[35] = '20080000000000000000000000000000000'H
. . (Padding)paddingTx[0] = -
- Constraint:
car_StatusInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 02 00 80 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00

- No.: 2305
- Timestamp: 20:44:19:611_1
- RFN: 4402
- Chip: 4608
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2308
- Timestamp: 20:44:19:617_0
- RFN: 4402
- Chip: 29184
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000111'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '750DD49DE9CE9E430AD448A14575D8'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 3d 1e 75 0d d4 9d e9 ce 9e 43 0a d4 48 a1 45 75 d8

- No.: 2324
- Timestamp: 20:44:19:651_0
- RFN: 4406
- Chip: 4864
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: tc_7_2_3_14:lt_ChkPollBitAndStatus LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. STATUS_PDU
. . (DC_Field)dC_Field[1] = '0'B
. . (CtrlPDU_Type)type[3] = '000'B
. . SuperFields
. . . SUFI_WindowSize
. . . SUFI_List
. . . SUFI_RList
. . . SUFI_Bitmap
. . . SUFI_MRW
. . . SUFI_MRW_ACK
. . . SUFI_NoMore
. . . SUFI_Ack
. . . . (SUFI_Type)type[4] = '0010'B
. . . . (AM_SeqNum)lsn[12] = '000000001000'B
. . (HexStringType)superFieldsAndPadRx[-1] = -
. . (Padding)paddingTx[-1] = '0000000000000000000000000000000'H
- Constraint:
cas_StatusReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 02 00 80 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00

- No.: 2327
- Timestamp: 20:44:19:653_1
- RFN: 4406
- Chip: 11776
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2330
- Timestamp: 20:44:19:656_1
- RFN: 4406
- Chip: 23040
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 2359
- Timestamp: 20:44:19:714_0
- RFN: 4412
- Chip: 15616
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000010001'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '9C160255088140200555DDC9CBCB9E'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 8d 1e 9c 16 02 55 08 81 40 20 05 55 dd c9 cb cb 9e

- No.: 2368
- Timestamp: 20:44:19:727_0
- RFN: 4413
- Chip: 28416
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 2369
- Timestamp: 20:44:19:727_1
- RFN: 4413
- Chip: 29184
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2374
- Timestamp: 20:44:19:745_0
- RFN: 4415
- Chip: 20224
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 2383
- Timestamp: 20:44:19:762_1
- RFN: 4417
- Chip: 11520
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 14
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 2384
- Timestamp: 20:44:19:763_0
- RFN: 4417
- Chip: 12544
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2389
- Timestamp: 20:44:19:785_1
- RFN: 4419
- Chip: 20736
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 2398
- Timestamp: 20:44:19:802_1
- RFN: 4421
- Chip: 11520
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 14
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 2399
- Timestamp: 20:44:19:803_0
- RFN: 4421
- Chip: 12544
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2404
- Timestamp: 20:44:19:825_0
- RFN: 4423
- Chip: 21248
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 2413
- Timestamp: 20:44:19:843_0
- RFN: 4425
- Chip: 13056
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 14
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 2414
- Timestamp: 20:44:19:843_1
- RFN: 4425
- Chip: 13824
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2419
- Timestamp: 20:44:19:865_1
- RFN: 4427
- Chip: 24064
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 2428
- Timestamp: 20:44:19:885_0
- RFN: 4429
- Chip: 22528
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 14
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 2429
- Timestamp: 20:44:19:885_1
- RFN: 4429
- Chip: 23296
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2432
- Timestamp: 20:44:19:898_0
- RFN: 4430
- Chip: 29696
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 5
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. STATUS_PDU
. . (DC_Field)dC_Field[1] = '0'B
. . (CtrlPDU_Type)type[3] = '000'B
. . SuperFields
. . (HexStringType)superFieldsAndPadRx[35] = '20080000000000000000000000000000000'H
. . (Padding)paddingTx[0] = -
- Constraint:
car_StatusInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 02 00 80 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00

- No.: 2434
- Timestamp: 20:44:19:901_1
- RFN: 4431
- Chip: 5120
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2439
- Timestamp: 20:44:19:907_1
- RFN: 4431
- Chip: 25856
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 2465
- Timestamp: 20:44:19:952_0
- RFN: 4436
- Chip: 8704
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000001000'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '9C160255088140200555DDC9CBCB9E'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 41 1e 9c 16 02 55 08 81 40 20 05 55 dd c9 cb cb 9e

- No.: 2474
- Timestamp: 20:44:19:966_0
- RFN: 4437
- Chip: 22528
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 2475
- Timestamp: 20:44:19:966_1
- RFN: 4437
- Chip: 23552
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2480
- Timestamp: 20:44:19:986_0
- RFN: 4439
- Chip: 23296
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 2488
- Timestamp: 20:44:20:001_0
- RFN: 4441
- Chip: 4608
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 14
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 2489
- Timestamp: 20:44:20:001_1
- RFN: 4441
- Chip: 5632
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2494
- Timestamp: 20:44:20:016_1
- RFN: 4442
- Chip: 23808
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 2502
- Timestamp: 20:44:20:031_0
- RFN: 4444
- Chip: 4352
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 14
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 2503
- Timestamp: 20:44:20:031_1
- RFN: 4444
- Chip: 5120
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2508
- Timestamp: 20:44:20:046_1
- RFN: 4445
- Chip: 24064
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 2516
- Timestamp: 20:44:20:061_0
- RFN: 4447
- Chip: 4608
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 14
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 2517
- Timestamp: 20:44:20:061_1
- RFN: 4447
- Chip: 5376
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2522
- Timestamp: 20:44:20:076_0
- RFN: 4448
- Chip: 24064
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 2530
- Timestamp: 20:44:20:091_0
- RFN: 4450
- Chip: 4352
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 14
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 2531
- Timestamp: 20:44:20:091_1
- RFN: 4450
- Chip: 5376
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2536
- Timestamp: 20:44:20:106_1
- RFN: 4451
- Chip: 25600
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 2544
- Timestamp: 20:44:20:123_0
- RFN: 4453
- Chip: 13824
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 14
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 2545
- Timestamp: 20:44:20:123_1
- RFN: 4453
- Chip: 14592
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2548
- Timestamp: 20:44:20:130_0
- RFN: 4454
- Chip: 3840
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000001000'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '9C160255088140200555DDC9CBCB9E'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 45 1e 9c 16 02 55 08 81 40 20 05 55 dd c9 cb cb 9e

- No.: 2566
- Timestamp: 20:44:20:158_1
- RFN: 4456
- Chip: 35328
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 8
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2568
- Timestamp: 20:44:20:162_1
- RFN: 4457
- Chip: 10496
- Event: Cancel Timer
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 9
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 2572
- Timestamp: 20:44:20:170_0
- RFN: 4458
- Chip: 4864
- Event: Send
- PCO: Dc
- Message: RRC_DataReq
- Source: ts_TC_OpenUE_TestLoop LINE 6
- Message Structure:
RRC_DataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[-1] = -
. (SapId)sapId[1] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. OPENUETESTLOOP
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)tCProtocolDiscriminator[4] = '1111'B
. . (MsgType)msgType[8] = '01000010'B
- Constraint:
ca_PS_DataReq
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 0f 42

- No.: 2573
- Timestamp: 20:44:20:171_0
- RFN: 4458
- Chip: 8448
- Event: Start Timer
- Source: ts_TC_OpenUE_TestLoop LINE 6
- Message Structure:
no details available
- Constraint:
t_Dly (5000 Ms)
- BinaryMessage:

- No.: 2577
- Timestamp: 20:44:20:453_0
- RFN: 4486
- Chip: 12544
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_TC_OpenUE_TestLoop LINE 7
- Message Structure:
RRC_DataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. (START_Value)start[0] = -
. OPENUETESTLOOPCOMPLETE
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)tCProtocolDiscriminator[4] = '1111'B
. . (MsgType)msgType[8] = '01000011'B
- Constraint:
car_PS_UplinkDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 0f 43

- No.: 2578
- Timestamp: 20:44:20:453_1
- RFN: 4486
- Chip: 15616
- Event: Cancel Timer
- Source: ts_TC_OpenUE_TestLoop LINE 7
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 2579
- Timestamp: 20:44:20:454_0
- RFN: 4486
- Chip: 16640
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_TC_OpenUE_TestLoop LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2597
- Timestamp: 20:44:20:479_0
- RFN: 4488
- Chip: 37632
- Event: Send
- PCO: CPHY
- Message: CPHY_Frame_Number_REQ
- Source: ts_CPHY_ActTime LINE 1
- Message Structure:
CPHY_Frame_Number_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
cas_GetFrameNum
- BinaryMessage:
30 06 02 01 00 02 01 1a

- No.: 2601
- Timestamp: 20:44:20:488_0
- RFN: 4489
- Chip: 34304
- Event: Receive
- PCO: CPHY
- Message: CPHY_Frame_Number_CNF
- Source: ts_CPHY_ActTime LINE 2
- Message Structure:
CPHY_Frame_Number_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
. (IntegerType)frameNumber = 137
- Constraint:
car_GetFrameNum
- BinaryMessage:
30 0a 02 01 00 02 01 1a 02 02 00 89

- No.: 2607
- Timestamp: 20:44:20:537_0
- RFN: 4494
- Chip: 25600
- Event: Send
- PCO: AM
- Message: RLC_AM_DATA_REQ
- Source: ts_RRC_RB_RelRLC:lt_SendRAB_Rel LINE 4
- Message Structure:
RLC_AM_DATA_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. AmConfirmationRequest
. aM_message
. . DL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00000000000000000000000000000000"
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . DL_DCCH_MessageType
. . . . RadioBearerRelease
. . . . . r3
. . . . . . RadioBearerRelease_r3_IEs
. . . . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . . . IntegrityProtectionModeInfo
. . . . . . . CipheringModeInfo
. . . . . . . (IntegerType)activationTime = 128
. . . . . . . U_RNTI
. . . . . . . (BitStringType)new_C_RNTI[16] = -
. . . . . . . (RRC_StateIndicator)rrc_StateIndicator = 0
. . . . . . . (IntegerType)utran_DRX_CycleLengthCoeff = -
. . . . . . . CN_InformationInfo
. . . . . . . (CN_DomainIdentity)signallingConnectionRelIndication = -
. . . . . . . (BitStringType)ura_Identity[16] = -
. . . . . . . RAB_InformationReconfigList
. . . . . . . RB_InformationReleaseList
. . . . . . . . (IntegerType)_elem = 20
. . . . . . . RB_InformationAffectedList
. . . . . . . DL_CounterSynchronisationInfo
. . . . . . . UL_CommonTransChInfo
. . . . . . . . TFC_Subset
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . TFCS
. . . . . . . . . . . ExplicitTFCS_Configuration
. . . . . . . . . . . . TFCS_ReconfAdd
. . . . . . . . . . . . . ctfcSize
. . . . . . . . . . . . . . ctfc2Bit
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . . . . . . . (IntegerType)ctfc2 = 0
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . . . . . . . (IntegerType)ctfc2 = 1
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 11
. . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . UL_DeletedTransChInfoList
. . . . . . . . UL_TransportChannelIdentity
. . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType = 0
. . . . . . . . . (IntegerType)ul_TransportChannelIdentity = 1
. . . . . . . UL_AddReconfTransChInfoList
. . . . . . . . UL_AddReconfTransChInformation
. . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType = 0
. . . . . . . . . (IntegerType)transportChannelIdentity = 5
. . . . . . . . . TransportFormatSet
. . . . . . . . . . DedicatedTransChTFS
. . . . . . . . . . . tti
. . . . . . . . . . . . DedicatedDynamicTF_InfoList
. . . . . . . . . . . . . DedicatedDynamicTF_Info
. . . . . . . . . . . . . . rlc_Size
. . . . . . . . . . . . . . . BitModeRLC_SizeInfo
. . . . . . . . . . . . . . . . sizeType2
. . . . . . . . . . . . . . . . . (IntegerType)part1 = 2
. . . . . . . . . . . . . . . . . (IntegerType)part2 = -
. . . . . . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . LogicalChannelList
. . . . . . . . . . . SemistaticTF_Information
. . . . . . . . . . . . ChannelCodingType
. . . . . . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . . . . . (IntegerType)rateMatchingAttribute = 192
. . . . . . . . . . . . (CRC_Size)crc_Size = 3
. . . . . . . modeSpecificTransChInfo
. . . . . . . . fdd
. . . . . . . . . (IntegerType)cpch_SetID = -
. . . . . . . . . DRAC_StaticInformationList
. . . . . . . DL_CommonTransChInfo
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . dl_Parameters
. . . . . . . DL_DeletedTransChInfoList
. . . . . . . . DL_TransportChannelIdentity
. . . . . . . . . (DL_TrCH_Type)dl_TransportChannelType = 0
. . . . . . . . . (IntegerType)dl_TransportChannelIdentity = 6
. . . . . . . DL_AddReconfTransChInfo2List
. . . . . . . . DL_AddReconfTransChInformation2
. . . . . . . . . (DL_TrCH_Type)dl_TransportChannelType = 0
. . . . . . . . . (IntegerType)transportChannelIdentity = 10
. . . . . . . . . tfs_SignallingMode
. . . . . . . . . . UL_TransportChannelIdentity
. . . . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType = 0
. . . . . . . . . . . (IntegerType)ul_TransportChannelIdentity = 5
. . . . . . . . . QualityTarget
. . . . . . . FrequencyInfo
. . . . . . . . modeSpecificInfo
. . . . . . . . . FrequencyInfoFDD
. . . . . . . . . . (IntegerType)uarfcn_UL = -
. . . . . . . . . . (IntegerType)uarfcn_DL = 10700
. . . . . . . (IntegerType)maxAllowedUL_TX_Power = 33
. . . . . . . UL_ChannelRequirement
. . . . . . . . UL_DPCH_Info
. . . . . . . . . UL_DPCH_PowerControlInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (IntegerType)dpcch_PowerOffset = -40
. . . . . . . . . . . (IntegerType)pc_Preamble = 1
. . . . . . . . . . . (IntegerType)sRB_delay = 7
. . . . . . . . . . . PowerControlAlgorithm
. . . . . . . . . . . . (IntegerType)algorithm1 = 1
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (ScramblingCodeType)scramblingCodeType = 1
. . . . . . . . . . . (IntegerType)scramblingCode = 0
. . . . . . . . . . . (IntegerType)numberOfDPDCH = -
. . . . . . . . . . . (SpreadingFactor)spreadingFactor = 4
. . . . . . . . . . . (BooleanType)tfci_Existence = TRUE
. . . . . . . . . . . (IntegerType)numberOfFBI_Bits = -
. . . . . . . . . . . (PuncturingLimit)puncturingLimit = 15
. . . . . . . modeSpecificPhysChInfo
. . . . . . . . fdd
. . . . . . . . . DL_PDSCH_Information
. . . . . . . DL_CommonInformation
. . . . . . . . DL_DPCH_InfoCommon
. . . . . . . . . cfnHandling
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . DL_DPCH_PowerControlInfo
. . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . (DPC_Mode)dpc_Mode = 0
. . . . . . . . . . . (IntegerType)powerOffsetPilot_pdpdch = 0
. . . . . . . . . . . Dl_rate_matching_restriction
. . . . . . . . . . . SF512_AndPilot
. . . . . . . . . . . . (PilotBits128)sfd128 = 0
. . . . . . . . . . . (PositionFixedOrFlexible)positionFixedOrFlexible = 0
. . . . . . . . . . . (BooleanType)tfci_Existence = FALSE
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . (IntegerType)defaultDPCH_OffsetValue = -
. . . . . . . . . . DPCH_CompressedModeInfo
. . . . . . . . . . (TX_DiversityMode)tx_DiversityMode = 0
. . . . . . . . . . SSDT_Information
. . . . . . . DL_InformationPerRL_List
. . . . . . . . DL_InformationPerRL
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . PrimaryCPICH_Info
. . . . . . . . . . . . (IntegerType)primaryScramblingCode = 100
. . . . . . . . . . . PDSCH_SHO_DCH_Info
. . . . . . . . . . . PDSCH_CodeMapping
. . . . . . . . . DL_DPCH_InfoPerRL
. . . . . . . . . . fdd
. . . . . . . . . . . (PCPICH_UsageForChannelEst)pCPICH_UsageForChannelEst = 0
. . . . . . . . . . . (IntegerType)dpch_FrameOffset = 0
. . . . . . . . . . . SecondaryCPICH_Info
. . . . . . . . . . . DL_ChannelisationCodeList
. . . . . . . . . . . . DL_ChannelisationCode
. . . . . . . . . . . . . (IntegerType)secondaryScramblingCode = 1
. . . . . . . . . . . . . SF512_AndCodeNumber
. . . . . . . . . . . . . . (IntegerType)sf128 = 0
. . . . . . . . . . . . . (ScramblingCodeChange)scramblingCodeChange = -
. . . . . . . . . . . (IntegerType)tpc_CombinationIndex = 0
. . . . . . . . . . . (SSDT_CellIdentity)ssdt_CellIdentity = -
. . . . . . . . . . . (ClosedLoopTimingAdjMode)closedLoopTimingAdjMode = -
. . . . . . . . . SCCPCH_InfoForFACH
. . . . . . v3a0NonCriticalExtensions
. . . . . . . RadioBearerRelease_v3a0ext
. . . . . . . . (BitStringType)new_DSCH_RNTI[16] = -
. . . . . . . laterNonCriticalExtensions
- Constraint:
cas_RB_Release
- BinaryMessage:
30 3a 02 01 ff 02 01 02 05 00 80 00 00 00 03 52 00 ff f2 00 04 c8 00 06 25 2b f0 00 00 40 01 10 44 77 ec 18 05 00 98 85 39 94 d2 a3 d1 00 00 00 9f 24 02 81 02 06 40 00 08 28 00 00

- No.: 2618
- Timestamp: 20:44:20:554_0
- RFN: 4496
- Chip: 14080
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = -12
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 f4 0a 01 00 05 00

- No.: 2622
- Timestamp: 20:44:20:561_0
- RFN: 4497
- Chip: 4864
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = -12
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 f4

- No.: 2631
- Timestamp: 20:44:20:573_0
- RFN: 4498
- Chip: 12288
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Modify_REQ
- Source: ts_SS_1DCH_DCCH_Modify LINE 4
- Message Structure:
CPHY_RL_Modify_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
. (RatType)ratType = 0
. CphyRlModifyReq
. . SS_ActivationTime
. . . (IntegerType)activationCFN = 128
. . physicalChannelInfo
. . . DPCHInfo
. . . . UL_DPCH_Info
. . . . DL_DPCHInfo
. . . . . DL_CommonInformation
. . . . . . DL_DPCH_InfoCommon
. . . . . . . cfnHandling
. . . . . . . . initialise
. . . . . . . . . (IntegerType)cfntargetsfnframeoffset = -
. . . . . . . modeSpecificInfo
. . . . . . . . fdd
. . . . . . . . . DL_DPCH_PowerControlInfo
. . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . fdd
. . . . . . . . . . . . (DPC_Mode)dpc_Mode = 0
. . . . . . . . . (IntegerType)powerOffsetPilot_pdpdch = 0
. . . . . . . . . Dl_rate_matching_restriction
. . . . . . . . . SF512_AndPilot
. . . . . . . . . . (PilotBits128)sfd128 = 0
. . . . . . . . . (PositionFixedOrFlexible)positionFixedOrFlexible = 0
. . . . . . . . . (BooleanType)tfci_Existence = FALSE
. . . . . . modeSpecificInfo
. . . . . . . fdd
. . . . . . . . (IntegerType)defaultDPCH_OffsetValue = 0
. . . . . . . . DPCH_CompressedModeInfo
. . . . . . . . (TX_DiversityMode)tx_DiversityMode = 0
. . . . . . . . SSDT_Information
. . . . . DL_DPCH_InfoPerRL
. . . . . . fdd
. . . . . . . (PCPICH_UsageForChannelEst)pCPICH_UsageForChannelEst = 0
. . . . . . . (IntegerType)dpch_FrameOffset = 0
. . . . . . . SecondaryCPICH_Info
. . . . . . . DL_ChannelisationCodeList
. . . . . . . . DL_ChannelisationCode
. . . . . . . . . (IntegerType)secondaryScramblingCode = 1
. . . . . . . . . SF512_AndCodeNumber
. . . . . . . . . . (IntegerType)sf128 = 0
. . . . . . . . . (ScramblingCodeChange)scramblingCodeChange = -
. . . . . . . (IntegerType)tpc_CombinationIndex = 0
. . . . . . . (SSDT_CellIdentity)ssdt_CellIdentity = -
. . . . . . . (ClosedLoopTimingAdjMode)closedLoopTimingAdjMode = -
. . . . . (IntegerType)powerOffsetOfTFCI_PO1 = 0
. . . . . (IntegerType)powerOffsetOfTPC_PO2 = 0
. . . . . (IntegerType)powerOffsetOfPILOT_PO3 = 0
. . . . . (IntegerType)dl_TxPower = -5
. . . . . (IntegerType)dl_TxPowerMax = 15
. . . . . (IntegerType)dl_TxPowerMin = -35
- Constraint:
ca_DL_DPCH_ModifyInfo
- BinaryMessage:
30 62 02 01 00 02 01 1a 0a 01 00 30 57 02 02 00 80 30 51 30 4f 30 25 30 1a 30 30 00 30 30 14 30 06 30 30 03 0a 01 00 02 01 00 0a 01 00 0a 01 00 01 01 00 30 30 06 02 01 00 0a 01 00 30 30 13 0a 01 00 02 01 00 30 08 30 06 02 01 01 02 01 00 02 01 00 02 01 00 02 01 00 02 01 00 02 01 fb 02 01 0f 02 01 dd

- No.: 2635
- Timestamp: 20:44:20:580_0
- RFN: 4499
- Chip: 1024
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Modify_CNF
- Source: ts_SS_1DCH_DCCH_Modify LINE 5
- Message Structure:
CPHY_RL_Modify_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
ca_RL_ModifyCnf
- BinaryMessage:
30 06 02 01 00 02 01 1a

- No.: 2636
- Timestamp: 20:44:20:591_0
- RFN: 4500
- Chip: 5888
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Config_REQ
- Source: ts_SS_1DCH_DCCH_Modify LINE 6
- Message Structure:
CPHY_TrCH_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
. (RatType)ratType = 0
. CphyTrchConfigReq
. . SS_ActivationTime
. . . (IntegerType)activationCFN = 128
. . ulconnectedTrCHList
. . TFCS
. . dlconnectedTrCHList
. . . CphyTrchConfigReq_setseq_1
. . . . (IntegerType)trchid = 10
. . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 148
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional = 1
. . . . . . (IntegerType)rateMatchingAttribute = 192
. . . . . . (CRC_Size)crc_Size = 3
. . TFCS
. . . ExplicitTFCS_Configuration
. . . . TFCS_ReconfAdd
. . . . . ctfcSize
. . . . . . ctfc2Bit
. . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . (IntegerType)ctfc2 = 0
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . (IntegerType)ctfc2 = 1
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . fdd
. . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 11
. . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
- Constraint:
ca_DCH_148_TTI_10_DL_Info
- BinaryMessage:
30 5b 02 01 00 02 01 1a 0a 01 00 30 50 02 02 00 80 30 26 30 24 02 01 0a 0a 01 00 30 1c 30 0e 30 0c 02 02 00 94 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 c0 0a 01 03 30 22 30 30 1f 30 08 02 01 00 30 03 02 01 00 30 13 02 01 01 30 0e 30 0c 30 30 03 02 01 0b 02 01 0f 02 01 00

- No.: 2640
- Timestamp: 20:44:20:603_0
- RFN: 4501
- Chip: 11776
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Config_CNF
- Source: ts_SS_1DCH_DCCH_Modify LINE 7
- Message Structure:
CPHY_TrCH_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
ca_TrChCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 1a

- No.: 2641
- Timestamp: 20:44:20:645_0
- RFN: 4505
- Chip: 19968
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_SS_1DCH_DCCH_Modify LINE 8
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
. (RatType)ratType = 0
. configMessage
. . CmacConfigReq
. . . SS_ActivationTime
. . . . (IntegerType)activationCFN = 128
. . . UE_Info
. . . . U_RNTI
. . . . (BitStringType)c_RNTI[16] = -
. . . TrCHInfo
. . . . ulconnectedTrCHList
. . . . TFCS
. . . . dlconnectedTrCHList
. . . . . TrCHInfo_setseq_1
. . . . . . (IntegerType)trchid = 10
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 148
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . (IntegerType)rateMatchingAttribute = 192
. . . . . . . . (CRC_Size)crc_Size = 3
. . . . TFCS
. . . . . ExplicitTFCS_Configuration
. . . . . . TFCS_ReconfAdd
. . . . . . . ctfcSize
. . . . . . . . ctfc2Bit
. . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . (IntegerType)ctfc2 = 0
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . (IntegerType)ctfc2 = 1
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 11
. . . . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . TrCH_LogCHMappingList1
. . . . ulconnectedTrCHList
. . . . dlconnectedTrCHList
. . . . . TrCH_LogCHMappingList1_setseq_1
. . . . . . (IntegerType)trchid = 10
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 1
. . . . . . . . (IntegerType)rB_Identity = 1
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 2
. . . . . . . . (IntegerType)rB_Identity = 2
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 3
. . . . . . . . (IntegerType)rB_Identity = 3
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 4
. . . . . . . . (IntegerType)rB_Identity = 4
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_CMAC_ReconfigInfo
- BinaryMessage:
30 81 c8 02 01 ff 02 01 1a 0a 01 00 30 81 bc 02 02 00 80 30 00 30 49 30 23 30 21 02 01 0a 30 1c 30 0e 30 0c 02 02 00 94 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 c0 0a 01 03 30 22 30 30 1f 30 08 02 01 00 30 03 02 01 00 30 13 02 01 01 30 0e 30 0c 30 30 03 02 01 0b 02 01 0f 02 01 00 30 69 30 67 30 65 02 01 0a 30 60 30 16 30 11 0a 01 00 0a 01 00 02 01 01 0a 01 04 05 00 02 01 01 02 01 01 30 16 30 11 0a 01 00 0a 01 00 02 01 02 0a 01 04 05 00 02 01 02 02 01 02 30 16 30 11 0a 01 00 0a 01 00 02 01 03 0a 01 04 05 00 02 01 03 02 01 03 30 16 30 11 0a 01 00 0a 01 00 02 01 04 0a 01 04 05 00 02 01 04 02 01 04

- No.: 2642
- Timestamp: 20:44:20:654_0
- RFN: 4506
- Chip: 16896
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_SS_1DCH_DCCH_Modify LINE 9
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 1a

- No.: 2643
- Timestamp: 20:44:20:660_0
- RFN: 4507
- Chip: 1792
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Modify_REQ
- Source: ts_SS_1DCH_DCCH_Modify LINE 10
- Message Structure:
CPHY_RL_Modify_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
. (RatType)ratType = 0
. CphyRlModifyReq
. . SS_ActivationTime
. . . (IntegerType)activationCFN = 128
. . physicalChannelInfo
. . . DPCHInfo
. . . . UL_DPCH_Info
. . . . . UL_DPCH_PowerControlInfo
. . . . . . fdd
. . . . . . . (IntegerType)dpcch_PowerOffset = -40
. . . . . . . (IntegerType)pc_Preamble = 1
. . . . . . . (IntegerType)sRB_delay = 7
. . . . . . . PowerControlAlgorithm
. . . . . . . . (IntegerType)algorithm1 = 1
. . . . . modeSpecificInfo
. . . . . . fdd
. . . . . . . (ScramblingCodeType)scramblingCodeType = 1
. . . . . . . (IntegerType)scramblingCode = 0
. . . . . . . (IntegerType)numberOfDPDCH = -
. . . . . . . (SpreadingFactor)spreadingFactor = 4
. . . . . . . (BooleanType)tfci_Existence = TRUE
. . . . . . . (IntegerType)numberOfFBI_Bits = -
. . . . . . . (PuncturingLimit)puncturingLimit = 15
. . . . DL_DPCHInfo
- Constraint:
ca_UL_DPCH_ModifyInfo
- BinaryMessage:
30 34 02 01 00 02 01 14 0a 01 00 30 29 02 02 00 80 30 23 30 21 30 30 0c 02 01 d8 02 01 01 02 01 07 02 01 01 30 30 0f 0a 01 01 02 01 00 0a 01 04 01 01 ff 0a 01 0f

- No.: 2647
- Timestamp: 20:44:20:670_0
- RFN: 4508
- Chip: 1792
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Modify_CNF
- Source: ts_SS_1DCH_DCCH_Modify LINE 11
- Message Structure:
CPHY_RL_Modify_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_RL_ModifyCnf
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 2648
- Timestamp: 20:44:20:679_0
- RFN: 4508
- Chip: 36864
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Config_REQ
- Source: ts_SS_1DCH_DCCH_Modify LINE 12
- Message Structure:
CPHY_TrCH_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
. (RatType)ratType = 0
. CphyTrchConfigReq
. . SS_ActivationTime
. . . (IntegerType)activationCFN = 128
. . ulconnectedTrCHList
. . . CphyTrchConfigReq_setseq_0
. . . . (IntegerType)trchid = 5
. . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 148
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional = 1
. . . . . . (IntegerType)rateMatchingAttribute = 192
. . . . . . (CRC_Size)crc_Size = 3
. . TFCS
. . . ExplicitTFCS_Configuration
. . . . TFCS_ReconfAdd
. . . . . ctfcSize
. . . . . . ctfc2Bit
. . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . (IntegerType)ctfc2 = 0
. . . . . . . . PowerOffsetInformation
. . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . (IntegerType)ctfc2 = 1
. . . . . . . . PowerOffsetInformation
. . dlconnectedTrCHList
. . TFCS
- Constraint:
ca_DCH_148_TTI_10_UL_Info
- BinaryMessage:
30 46 02 01 00 02 01 14 0a 01 00 30 3b 02 02 00 80 30 26 30 24 02 01 05 0a 01 00 30 1c 30 0e 30 0c 02 02 00 94 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 c0 0a 01 03 30 0d 30 30 0a 30 03 02 01 00 30 03 02 01 01

- No.: 2652
- Timestamp: 20:44:20:692_0
- RFN: 4510
- Chip: 8960
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Config_CNF
- Source: ts_SS_1DCH_DCCH_Modify LINE 13
- Message Structure:
CPHY_TrCH_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_TrChCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 2653
- Timestamp: 20:44:20:728_0
- RFN: 4513
- Chip: 33280
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_SS_1DCH_DCCH_Modify LINE 14
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
. (RatType)ratType = 0
. configMessage
. . CmacConfigReq
. . . SS_ActivationTime
. . . . (IntegerType)activationCFN = 128
. . . UE_Info
. . . . U_RNTI
. . . . (BitStringType)c_RNTI[16] = -
. . . TrCHInfo
. . . . ulconnectedTrCHList
. . . . . TrCHInfo_setseq_0
. . . . . . (IntegerType)trchid = 5
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 148
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . (IntegerType)rateMatchingAttribute = 192
. . . . . . . . (CRC_Size)crc_Size = 3
. . . . TFCS
. . . . . ExplicitTFCS_Configuration
. . . . . . TFCS_ReconfAdd
. . . . . . . ctfcSize
. . . . . . . . ctfc2Bit
. . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . (IntegerType)ctfc2 = 0
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . (IntegerType)ctfc2 = 1
. . . . . . . . . . PowerOffsetInformation
. . . . dlconnectedTrCHList
. . . . TFCS
. . . TrCH_LogCHMappingList1
. . . . ulconnectedTrCHList
. . . . . TrCH_LogCHMappingList1_setseq_0
. . . . . . (IntegerType)trchid = 5
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . (IntegerType)rB_Identity = 1
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . (IntegerType)rB_Identity = 2
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . (IntegerType)rB_Identity = 3
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . (IntegerType)rB_Identity = 4
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . dlconnectedTrCHList
- Constraint:
ca_CMAC_ReconfigInfo
- BinaryMessage:
30 81 9f 02 01 ff 02 01 14 0a 01 00 30 81 93 02 02 00 80 30 00 30 34 30 23 30 21 02 01 05 30 1c 30 0e 30 0c 02 02 00 94 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 c0 0a 01 03 30 0d 30 30 0a 30 03 02 01 00 30 03 02 01 01 30 55 30 53 30 51 02 01 05 30 4c 30 11 30 0c 0a 01 00 0a 01 00 02 01 01 0a 01 04 02 01 01 30 11 30 0c 0a 01 00 0a 01 00 02 01 02 0a 01 04 02 01 02 30 11 30 0c 0a 01 00 0a 01 00 02 01 03 0a 01 04 02 01 03 30 11 30 0c 0a 01 00 0a 01 00 02 01 04 0a 01 04 02 01 04

- No.: 2657
- Timestamp: 20:44:20:737_0
- RFN: 4514
- Chip: 28928
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_SS_1DCH_DCCH_Modify LINE 15
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 14

- No.: 2667
- Timestamp: 20:44:20:740_0
- RFN: 4515
- Chip: 1280
- Event: Start Timer
- Source: ts_RRC_ReceiveRB_RelCmpl LINE 2
- Message Structure:
no details available
- Constraint:
t_WaitMS (13500 Ms)
- BinaryMessage:

- No.: 2671
- Timestamp: 20:44:23:012_0
- RFN: 4742
- Chip: 10496
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_IND
- Source: ts_RRC_ReceiveRB_RelCmpl LINE 3
- Message Structure:
RLC_AM_DATA_IND
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. IntegrityResult
. . (IntegrityStatus)integrityUsed = 0
. aM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "11100111101110000111111101010101"
. . . . (IntegerType)rrc_MessageSequenceNumber = 3
. . . UL_DCCH_MessageType
. . . . RadioBearerReleaseComplete
. . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . IntegrityProtActivationInfo
. . . . . (IntegerType)ul_TimingAdvance = 0
. . . . . (IntegerType)count_C_ActivationTime = 0
. . . . . UL_CounterSynchronisationInfo
. . . . . laterNonCriticalExtensions
. . . . . . (BitStringType)radioBearerReleaseComplete_r3_add_ext = 0
. . . . . . nonCriticalExtensions
- Constraint:
car_RB_RelCmpl
- BinaryMessage:
30 10 02 01 ff 02 01 02 0a 01 00 f3 dc 3f aa 9b 40 00

- No.: 2672
- Timestamp: 20:44:23:013_0
- RFN: 4742
- Chip: 15104
- Event: Cancel Timer
- Source: ts_RRC_ReceiveRB_RelCmpl LINE 3
- Message Structure:
no details available
- Constraint:
t_WaitMS
- BinaryMessage:

- No.: 2673
- Timestamp: 20:44:23:013_1
- RFN: 4742
- Chip: 16128
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ReceiveRB_RelCmpl LINE 3
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2702
- Timestamp: 20:44:23:042_0
- RFN: 4745
- Chip: 9216
- Event: Send
- PCO: CPHY
- Message: CPHY_Frame_Number_REQ
- Source: ts_RRC_SetUpRAB_AM_7_RLC LINE 2
- Message Structure:
CPHY_Frame_Number_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
cas_GetFrameNum
- BinaryMessage:
30 06 02 01 00 02 01 1a

- No.: 2706
- Timestamp: 20:44:23:052_0
- RFN: 4746
- Chip: 9216
- Event: Receive
- PCO: CPHY
- Message: CPHY_Frame_Number_CNF
- Source: ts_RRC_SetUpRAB_AM_7_RLC LINE 3
- Message Structure:
CPHY_Frame_Number_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
. (IntegerType)frameNumber = 137
- Constraint:
car_GetFrameNum
- BinaryMessage:
30 0a 02 01 00 02 01 1a 02 02 00 89

- No.: 2710
- Timestamp: 20:44:23:098_0
- RFN: 4750
- Chip: 32512
- Event: Send
- PCO: AM
- Message: RLC_AM_DATA_REQ
- Source: ts_RRC_SetUpRAB_AM_7_RLC:lt_SendRAB_SetupCS_OrPS LINE 4
- Message Structure:
RLC_AM_DATA_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. AmConfirmationRequest
. . (IntegerType)confirmationRequested = 0
. aM_message
. . DL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00000000000000000000000000000000"
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . DL_DCCH_MessageType
. . . . RadioBearerSetup
. . . . . r3
. . . . . . RadioBearerSetup_r3_IEs
. . . . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . . . IntegrityProtectionModeInfo
. . . . . . . CipheringModeInfo
. . . . . . . (IntegerType)activationTime = 128
. . . . . . . U_RNTI
. . . . . . . (BitStringType)new_C_RNTI[16] = -
. . . . . . . (RRC_StateIndicator)rrc_StateIndicator = 0
. . . . . . . (IntegerType)utran_DRX_CycleLengthCoeff = -
. . . . . . . (BitStringType)ura_Identity[0] = -
. . . . . . . CN_InformationInfo
. . . . . . . SRB_InformationSetupList
. . . . . . . RAB_InformationSetupList
. . . . . . . . RAB_InformationSetup
. . . . . . . . . RAB_Info
. . . . . . . . . . RAB_Identity
. . . . . . . . . . . (BitStringType)gsm_MAP_RAB_Identity[8] = '00000101'B
. . . . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = 1
. . . . . . . . . . (BitStringType)nas_Synchronisation_Indicator[0] = -
. . . . . . . . . . (Re_EstablishmentTimer)re_EstablishmentTimer = 0
. . . . . . . . . RB_InformationSetupList
. . . . . . . . . . RB_InformationSetup
. . . . . . . . . . . (IntegerType)rb_Identity = 20
. . . . . . . . . . . PDCP_Info
. . . . . . . . . . . RLC_InfoChoice
. . . . . . . . . . . . RLC_Info
. . . . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . . . MaxDAT_Retransmissions
. . . . . . . . . . . . . . . . . (MaxDAT)maxDAT = 3
. . . . . . . . . . . . . . . . . (TimerMRW)timerMRW = 13
. . . . . . . . . . . . . . . . . (MaxMRW)maxMRW = 1
. . . . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize = 5
. . . . . . . . . . . . . . . (TimerRST)timerRST = 9
. . . . . . . . . . . . . . . (MaxRST)max_RST = 1
. . . . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit = -
. . . . . . . . . . . . . . . . (TimerPoll)timerPoll = -
. . . . . . . . . . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . . . . . . . . . (Poll_SDU)poll_SDU = -
. . . . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . . . (PollWindow)pollWindow = -
. . . . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize = 5
. . . . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit = -
. . . . . . . . . . . . . . . . (TimerEPC)timerEPC = -
. . . . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = FALSE
. . . . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . . . . . . . . RB_MappingInfo
. . . . . . . . . . . . RB_MappingOption
. . . . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . . . (IntegerType)dch = 1
. . . . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 7
. . . . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 7
. . . . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . . . (IntegerType)dch = 6
. . . . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 7
. . . . . . . RB_InformationAffectedList
. . . . . . . DL_CounterSynchronisationInfo
. . . . . . . UL_CommonTransChInfo
. . . . . . . . TFC_Subset
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . TFCS
. . . . . . . . . . . ExplicitTFCS_Configuration
. . . . . . . . . . . . TFCS_ReconfAdd
. . . . . . . . . . . . . ctfcSize
. . . . . . . . . . . . . . ctfc4Bit
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . . . . . . . (IntegerType)ctfc4 = 0
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . . . . . . . (IntegerType)ctfc4 = 1
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . . . . . . . (IntegerType)ctfc4 = 2
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . . . . . . . (IntegerType)ctfc4 = 3
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 11
. . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . UL_DeletedTransChInfoList
. . . . . . . UL_AddReconfTransChInfoList
. . . . . . . . UL_AddReconfTransChInformation
. . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType = 0
. . . . . . . . . (IntegerType)transportChannelIdentity = 1
. . . . . . . . . TransportFormatSet
. . . . . . . . . . DedicatedTransChTFS
. . . . . . . . . . . tti
. . . . . . . . . . . . DedicatedDynamicTF_InfoList
. . . . . . . . . . . . . DedicatedDynamicTF_Info
. . . . . . . . . . . . . . rlc_Size
. . . . . . . . . . . . . . . OctetModeRLC_SizeInfoType1
. . . . . . . . . . . . . . . . (IntegerType)sizeType1 = 16
. . . . . . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . LogicalChannelList
. . . . . . . . . . . SemistaticTF_Information
. . . . . . . . . . . . ChannelCodingType
. . . . . . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . . . . . (IntegerType)rateMatchingAttribute = 155
. . . . . . . . . . . . (CRC_Size)crc_Size = 3
. . . . . . . . UL_AddReconfTransChInformation
. . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType = 0
. . . . . . . . . (IntegerType)transportChannelIdentity = 5
. . . . . . . . . TransportFormatSet
. . . . . . . . . . DedicatedTransChTFS
. . . . . . . . . . . tti
. . . . . . . . . . . . DedicatedDynamicTF_InfoList
. . . . . . . . . . . . . DedicatedDynamicTF_Info
. . . . . . . . . . . . . . rlc_Size
. . . . . . . . . . . . . . . BitModeRLC_SizeInfo
. . . . . . . . . . . . . . . . sizeType2
. . . . . . . . . . . . . . . . . (IntegerType)part1 = 2
. . . . . . . . . . . . . . . . . (IntegerType)part2 = -
. . . . . . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . LogicalChannelList
. . . . . . . . . . . SemistaticTF_Information
. . . . . . . . . . . . ChannelCodingType
. . . . . . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . . . . . (IntegerType)rateMatchingAttribute = 170
. . . . . . . . . . . . (CRC_Size)crc_Size = 3
. . . . . . . modeSpecificTransChInfo
. . . . . . . . fdd
. . . . . . . . . (IntegerType)cpch_SetID = -
. . . . . . . . . DRAC_StaticInformationList
. . . . . . . DL_CommonTransChInfo
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . dl_Parameters
. . . . . . . DL_DeletedTransChInfoList
. . . . . . . DL_AddReconfTransChInfoList
. . . . . . . . DL_AddReconfTransChInformation
. . . . . . . . . (DL_TrCH_Type)dl_TransportChannelType = 0
. . . . . . . . . (IntegerType)dl_transportChannelIdentity = 6
. . . . . . . . . tfs_SignallingMode
. . . . . . . . . . UL_TransportChannelIdentity
. . . . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType = 0
. . . . . . . . . . . (IntegerType)ul_TransportChannelIdentity = 1
. . . . . . . . . QualityTarget
. . . . . . . . . . (IntegerType)bler_QualityValue = -20
. . . . . . . . . TM_SignallingInfo
. . . . . . . . DL_AddReconfTransChInformation
. . . . . . . . . (DL_TrCH_Type)dl_TransportChannelType = 0
. . . . . . . . . (IntegerType)dl_transportChannelIdentity = 10
. . . . . . . . . tfs_SignallingMode
. . . . . . . . . . UL_TransportChannelIdentity
. . . . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType = 0
. . . . . . . . . . . (IntegerType)ul_TransportChannelIdentity = 5
. . . . . . . . . QualityTarget
. . . . . . . . . . (IntegerType)bler_QualityValue = -20
. . . . . . . . . TM_SignallingInfo
. . . . . . . FrequencyInfo
. . . . . . . (IntegerType)maxAllowedUL_TX_Power = 33
. . . . . . . UL_ChannelRequirement
. . . . . . . . UL_DPCH_Info
. . . . . . . . . UL_DPCH_PowerControlInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (IntegerType)dpcch_PowerOffset = -40
. . . . . . . . . . . (IntegerType)pc_Preamble = 1
. . . . . . . . . . . (IntegerType)sRB_delay = 7
. . . . . . . . . . . PowerControlAlgorithm
. . . . . . . . . . . . (IntegerType)algorithm1 = 1
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (ScramblingCodeType)scramblingCodeType = 1
. . . . . . . . . . . (IntegerType)scramblingCode = 0
. . . . . . . . . . . (IntegerType)numberOfDPDCH = -
. . . . . . . . . . . (SpreadingFactor)spreadingFactor = 4
. . . . . . . . . . . (BooleanType)tfci_Existence = TRUE
. . . . . . . . . . . (IntegerType)numberOfFBI_Bits = -
. . . . . . . . . . . (PuncturingLimit)puncturingLimit = 15
. . . . . . . modeSpecificPhysChInfo
. . . . . . . . fdd
. . . . . . . . . DL_PDSCH_Information
. . . . . . . DL_CommonInformation
. . . . . . . . DL_DPCH_InfoCommon
. . . . . . . . . cfnHandling
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . DL_DPCH_PowerControlInfo
. . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . (DPC_Mode)dpc_Mode = 0
. . . . . . . . . . . (IntegerType)powerOffsetPilot_pdpdch = 0
. . . . . . . . . . . Dl_rate_matching_restriction
. . . . . . . . . . . SF512_AndPilot
. . . . . . . . . . . . (PilotBits128)sfd128 = 0
. . . . . . . . . . . (PositionFixedOrFlexible)positionFixedOrFlexible = 1
. . . . . . . . . . . (BooleanType)tfci_Existence = TRUE
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . (IntegerType)defaultDPCH_OffsetValue = -
. . . . . . . . . . DPCH_CompressedModeInfo
. . . . . . . . . . (TX_DiversityMode)tx_DiversityMode = 0
. . . . . . . . . . SSDT_Information
. . . . . . . DL_InformationPerRL_List
. . . . . . . . DL_InformationPerRL
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . PrimaryCPICH_Info
. . . . . . . . . . . . (IntegerType)primaryScramblingCode = 100
. . . . . . . . . . . PDSCH_SHO_DCH_Info
. . . . . . . . . . . PDSCH_CodeMapping
. . . . . . . . . DL_DPCH_InfoPerRL
. . . . . . . . . . fdd
. . . . . . . . . . . (PCPICH_UsageForChannelEst)pCPICH_UsageForChannelEst = 0
. . . . . . . . . . . (IntegerType)dpch_FrameOffset = 0
. . . . . . . . . . . SecondaryCPICH_Info
. . . . . . . . . . . DL_ChannelisationCodeList
. . . . . . . . . . . . DL_ChannelisationCode
. . . . . . . . . . . . . (IntegerType)secondaryScramblingCode = 1
. . . . . . . . . . . . . SF512_AndCodeNumber
. . . . . . . . . . . . . . (IntegerType)sf128 = 0
. . . . . . . . . . . . . (ScramblingCodeChange)scramblingCodeChange = -
. . . . . . . . . . . (IntegerType)tpc_CombinationIndex = 0
. . . . . . . . . . . (SSDT_CellIdentity)ssdt_CellIdentity = -
. . . . . . . . . . . (ClosedLoopTimingAdjMode)closedLoopTimingAdjMode = -
. . . . . . . . . SCCPCH_InfoForFACH
. . . . . . v3a0NonCriticalExtensions
. . . . . . . RadioBearerSetup_v3a0ext
. . . . . . . . (BitStringType)new_DSCH_RNTI[16] = -
. . . . . . . laterNonCriticalExtensions
- Constraint:
cas_RB_SetUpAM_WithCnf
- BinaryMessage:
30 4f 02 01 ff 02 01 02 02 01 00 80 00 00 00 03 92 04 ba f2 00 00 16 09 b3 1e 95 92 06 54 06 80 67 21 58 81 00 e0 91 49 24 ca fc 08 02 09 00 88 e6 98 84 02 20 88 ea 58 30 c2 c0 ae 26 25 74 d2 a3 d1 00 00 00 9f 24 02 b1 02 06 40 00 08 28 00 00

- No.: 2715
- Timestamp: 20:44:23:261_0
- RFN: 4767
- Chip: 7936
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_CNF
- Source: ts_RRC_SetUpRAB_AM_7_RLC LINE 6
- Message Structure:
RLC_AM_DATA_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. (IntegerType)mui = 0
- Constraint:
car_AM_DataMuiCnf
- BinaryMessage:
30 09 02 01 ff 02 01 02 02 01 00

- No.: 2722
- Timestamp: 20:44:23:397_0
- RFN: 4780
- Chip: 26624
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Modify_REQ
- Source: ts_SS_2DCH_Modify LINE 3
- Message Structure:
CPHY_RL_Modify_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
. (RatType)ratType = 0
. CphyRlModifyReq
. . SS_ActivationTime
. . . (IntegerType)activationCFN = 128
. . physicalChannelInfo
. . . DPCHInfo
. . . . UL_DPCH_Info
. . . . DL_DPCHInfo
. . . . . DL_CommonInformation
. . . . . . DL_DPCH_InfoCommon
. . . . . . . cfnHandling
. . . . . . . modeSpecificInfo
. . . . . . . . fdd
. . . . . . . . . DL_DPCH_PowerControlInfo
. . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . fdd
. . . . . . . . . . . . (DPC_Mode)dpc_Mode = 0
. . . . . . . . . (IntegerType)powerOffsetPilot_pdpdch = 0
. . . . . . . . . Dl_rate_matching_restriction
. . . . . . . . . SF512_AndPilot
. . . . . . . . . . (PilotBits128)sfd128 = 0
. . . . . . . . . (PositionFixedOrFlexible)positionFixedOrFlexible = 1
. . . . . . . . . (BooleanType)tfci_Existence = TRUE
. . . . . . modeSpecificInfo
. . . . . . . fdd
. . . . . . . . (IntegerType)defaultDPCH_OffsetValue = -
. . . . . . . . DPCH_CompressedModeInfo
. . . . . . . . (TX_DiversityMode)tx_DiversityMode = 0
. . . . . . . . SSDT_Information
. . . . . DL_DPCH_InfoPerRL
. . . . . . fdd
. . . . . . . (PCPICH_UsageForChannelEst)pCPICH_UsageForChannelEst = 0
. . . . . . . (IntegerType)dpch_FrameOffset = 0
. . . . . . . SecondaryCPICH_Info
. . . . . . . DL_ChannelisationCodeList
. . . . . . . . DL_ChannelisationCode
. . . . . . . . . (IntegerType)secondaryScramblingCode = 1
. . . . . . . . . SF512_AndCodeNumber
. . . . . . . . . . (IntegerType)sf128 = 0
. . . . . . . . . (ScramblingCodeChange)scramblingCodeChange = -
. . . . . . . (IntegerType)tpc_CombinationIndex = 0
. . . . . . . (SSDT_CellIdentity)ssdt_CellIdentity = -
. . . . . . . (ClosedLoopTimingAdjMode)closedLoopTimingAdjMode = -
. . . . . (IntegerType)powerOffsetOfTFCI_PO1 = 0
. . . . . (IntegerType)powerOffsetOfTPC_PO2 = 0
. . . . . (IntegerType)powerOffsetOfPILOT_PO3 = 0
. . . . . (IntegerType)dl_TxPower = -5
. . . . . (IntegerType)dl_TxPowerMax = 15
. . . . . (IntegerType)dl_TxPowerMin = -35
- Constraint:
ca_DL_DPCH_ModifyInfo
- BinaryMessage:
30 5e 02 01 00 02 01 1a 0a 01 00 30 53 02 02 00 80 30 4d 30 4b 30 21 30 19 05 00 30 30 14 30 06 30 30 03 0a 01 00 02 01 00 0a 01 00 0a 01 01 01 01 ff 30 30 03 0a 01 00 30 30 13 0a 01 00 02 01 00 30 08 30 06 02 01 01 02 01 00 02 01 00 02 01 00 02 01 00 02 01 00 02 01 fb 02 01 0f 02 01 dd

- No.: 2726
- Timestamp: 20:44:23:446_0
- RFN: 4785
- Chip: 22784
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Modify_CNF
- Source: ts_SS_2DCH_Modify LINE 4
- Message Structure:
CPHY_RL_Modify_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
ca_RL_ModifyCnf
- BinaryMessage:
30 06 02 01 00 02 01 1a

- No.: 2727
- Timestamp: 20:44:23:474_0
- RFN: 4788
- Chip: 16128
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Config_REQ
- Source: ts_SS_2DCH_Modify LINE 5
- Message Structure:
CPHY_TrCH_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
. (RatType)ratType = 0
. CphyTrchConfigReq
. . SS_ActivationTime
. . . (IntegerType)activationCFN = 128
. . ulconnectedTrCHList
. . TFCS
. . dlconnectedTrCHList
. . . CphyTrchConfigReq_setseq_1
. . . . (IntegerType)trchid = 6
. . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 144
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional = 1
. . . . . . (IntegerType)rateMatchingAttribute = 155
. . . . . . (CRC_Size)crc_Size = 3
. . . CphyTrchConfigReq_setseq_1
. . . . (IntegerType)trchid = 10
. . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 148
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional = 1
. . . . . . (IntegerType)rateMatchingAttribute = 170
. . . . . . (CRC_Size)crc_Size = 3
. . TFCS
. . . ExplicitTFCS_Configuration
. . . . TFCS_ReconfAdd
. . . . . ctfcSize
. . . . . . ctfc4Bit
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 0
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 1
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 2
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 3
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . fdd
. . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 9
. . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
- Constraint:
ca_TrChCfgInfo
- BinaryMessage:
30 81 96 02 01 00 02 01 1a 0a 01 00 30 81 8a 02 02 00 80 30 4c 30 24 02 01 06 0a 01 00 30 1c 30 0e 30 0c 02 02 00 90 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 9b 0a 01 03 30 24 02 01 0a 0a 01 00 30 1c 30 0e 30 0c 02 02 00 94 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 aa 0a 01 03 30 36 30 30 33 30 08 02 01 00 30 03 02 01 00 30 08 02 01 01 30 03 02 01 00 30 08 02 01 02 30 03 02 01 00 30 13 02 01 03 30 0e 30 0c 30 30 03 02 01 09 02 01 0f 02 01 00

- No.: 2731
- Timestamp: 20:44:23:524_0
- RFN: 4793
- Chip: 18176
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Config_CNF
- Source: ts_SS_2DCH_Modify LINE 6
- Message Structure:
CPHY_TrCH_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
ca_TrChCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 1a

- No.: 2732
- Timestamp: 20:44:23:581_0
- RFN: 4799
- Chip: 8192
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_SS_2DCH_Modify LINE 7
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
. (RatType)ratType = 0
. configMessage
. . CmacConfigReq
. . . SS_ActivationTime
. . . . (IntegerType)activationCFN = 128
. . . UE_Info
. . . . U_RNTI
. . . . (BitStringType)c_RNTI[16] = -
. . . TrCHInfo
. . . . ulconnectedTrCHList
. . . . TFCS
. . . . dlconnectedTrCHList
. . . . . TrCHInfo_setseq_1
. . . . . . (IntegerType)trchid = 6
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 144
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . (IntegerType)rateMatchingAttribute = 155
. . . . . . . . (CRC_Size)crc_Size = 3
. . . . . TrCHInfo_setseq_1
. . . . . . (IntegerType)trchid = 10
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 148
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . (IntegerType)rateMatchingAttribute = 170
. . . . . . . . (CRC_Size)crc_Size = 3
. . . . TFCS
. . . . . ExplicitTFCS_Configuration
. . . . . . TFCS_ReconfAdd
. . . . . . . ctfcSize
. . . . . . . . ctfc4Bit
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 0
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 1
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 2
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 3
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 9
. . . . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . TrCH_LogCHMappingList1
. . . . ulconnectedTrCHList
. . . . dlconnectedTrCHList
. . . . . TrCH_LogCHMappingList1_setseq_1
. . . . . . (IntegerType)trchid = 6
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 7
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 5
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 7
. . . . . . . . (IntegerType)rB_Identity = -12
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . TrCH_LogCHMappingList1_setseq_1
. . . . . . (IntegerType)trchid = 10
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 1
. . . . . . . . (IntegerType)rB_Identity = 1
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 2
. . . . . . . . (IntegerType)rB_Identity = 2
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 3
. . . . . . . . (IntegerType)rB_Identity = 3
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 4
. . . . . . . . (IntegerType)rB_Identity = 4
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_CMAC_ReconfigInfo
- BinaryMessage:
30 82 01 22 02 01 ff 02 01 1a 0a 01 00 30 82 01 15 02 02 00 80 30 00 30 81 80 30 46 30 21 02 01 06 30 1c 30 0e 30 0c 02 02 00 90 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 9b 0a 01 03 30 21 02 01 0a 30 1c 30 0e 30 0c 02 02 00 94 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 aa 0a 01 03 30 36 30 30 33 30 08 02 01 00 30 03 02 01 00 30 08 02 01 01 30 03 02 01 00 30 08 02 01 02 30 03 02 01 00 30 13 02 01 03 30 0e 30 0c 30 30 03 02 01 09 02 01 0f 02 01 00 30 81 89 30 81 86 30 1d 02 01 06 30 18 30 16 30 11 0a 01 00 0a 01 00 02 01 07 0a 01 05 05 00 02 01 07 02 01 f4 30 65 02 01 0a 30 60 30 16 30 11 0a 01 00 0a 01 00 02 01 01 0a 01 04 05 00 02 01 01 02 01 01 30 16 30 11 0a 01 00 0a 01 00 02 01 02 0a 01 04 05 00 02 01 02 02 01 02 30 16 30 11 0a 01 00 0a 01 00 02 01 03 0a 01 04 05 00 02 01 03 02 01 03 30 16 30 11 0a 01 00 0a 01 00 02 01 04 0a 01 04 05 00 02 01 04 02 01 04

- No.: 2736
- Timestamp: 20:44:23:635_0
- RFN: 4804
- Chip: 23296
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_SS_2DCH_Modify LINE 8
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 1a

- No.: 2737
- Timestamp: 20:44:23:662_0
- RFN: 4807
- Chip: 6400
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Modify_REQ
- Source: ts_SS_2DCH_Modify LINE 9
- Message Structure:
CPHY_RL_Modify_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
. (RatType)ratType = 0
. CphyRlModifyReq
. . SS_ActivationTime
. . . (IntegerType)activationCFN = 128
. . physicalChannelInfo
. . . DPCHInfo
. . . . UL_DPCH_Info
. . . . . UL_DPCH_PowerControlInfo
. . . . . . fdd
. . . . . . . (IntegerType)dpcch_PowerOffset = -40
. . . . . . . (IntegerType)pc_Preamble = 1
. . . . . . . (IntegerType)sRB_delay = 7
. . . . . . . PowerControlAlgorithm
. . . . . . . . (IntegerType)algorithm1 = 1
. . . . . modeSpecificInfo
. . . . . . fdd
. . . . . . . (ScramblingCodeType)scramblingCodeType = 1
. . . . . . . (IntegerType)scramblingCode = 0
. . . . . . . (IntegerType)numberOfDPDCH = -
. . . . . . . (SpreadingFactor)spreadingFactor = 4
. . . . . . . (BooleanType)tfci_Existence = TRUE
. . . . . . . (IntegerType)numberOfFBI_Bits = -
. . . . . . . (PuncturingLimit)puncturingLimit = 15
. . . . DL_DPCHInfo
- Constraint:
ca_UL_DPCH_ModifyInfo
- BinaryMessage:
30 34 02 01 00 02 01 14 0a 01 00 30 29 02 02 00 80 30 23 30 21 30 30 0c 02 01 d8 02 01 01 02 01 07 02 01 01 30 30 0f 0a 01 01 02 01 00 0a 01 04 01 01 ff 0a 01 0f

- No.: 2741
- Timestamp: 20:44:23:711_0
- RFN: 4812
- Chip: 3584
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Modify_CNF
- Source: ts_SS_2DCH_Modify LINE 10
- Message Structure:
CPHY_RL_Modify_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_RL_ModifyCnf
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 2742
- Timestamp: 20:44:23:738_0
- RFN: 4814
- Chip: 30464
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Config_REQ
- Source: ts_SS_2DCH_Modify LINE 11
- Message Structure:
CPHY_TrCH_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
. (RatType)ratType = 0
. CphyTrchConfigReq
. . SS_ActivationTime
. . . (IntegerType)activationCFN = 128
. . ulconnectedTrCHList
. . . CphyTrchConfigReq_setseq_0
. . . . (IntegerType)trchid = 1
. . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 144
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional = 1
. . . . . . (IntegerType)rateMatchingAttribute = 155
. . . . . . (CRC_Size)crc_Size = 3
. . . CphyTrchConfigReq_setseq_0
. . . . (IntegerType)trchid = 5
. . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 148
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional = 1
. . . . . . (IntegerType)rateMatchingAttribute = 170
. . . . . . (CRC_Size)crc_Size = 3
. . TFCS
. . . ExplicitTFCS_Configuration
. . . . TFCS_ReconfAdd
. . . . . ctfcSize
. . . . . . ctfc4Bit
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 0
. . . . . . . . PowerOffsetInformation
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 1
. . . . . . . . PowerOffsetInformation
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 2
. . . . . . . . PowerOffsetInformation
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 3
. . . . . . . . PowerOffsetInformation
. . dlconnectedTrCHList
. . TFCS
- Constraint:
ca_TrChCfgInfo
- BinaryMessage:
30 76 02 01 00 02 01 14 0a 01 00 30 6b 02 02 00 80 30 4c 30 24 02 01 01 0a 01 00 30 1c 30 0e 30 0c 02 02 00 90 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 9b 0a 01 03 30 24 02 01 05 0a 01 00 30 1c 30 0e 30 0c 02 02 00 94 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 aa 0a 01 03 30 17 30 30 14 30 03 02 01 00 30 03 02 01 01 30 03 02 01 02 30 03 02 01 03

- No.: 2746
- Timestamp: 20:44:23:787_0
- RFN: 4819
- Chip: 29696
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Config_CNF
- Source: ts_SS_2DCH_Modify LINE 12
- Message Structure:
CPHY_TrCH_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_TrChCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 2747
- Timestamp: 20:44:23:851_0
- RFN: 4826
- Chip: 7424
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_SS_2DCH_Modify LINE 13
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
. (RatType)ratType = 0
. configMessage
. . CmacConfigReq
. . . SS_ActivationTime
. . . . (IntegerType)activationCFN = 128
. . . UE_Info
. . . . U_RNTI
. . . . (BitStringType)c_RNTI[16] = -
. . . TrCHInfo
. . . . ulconnectedTrCHList
. . . . . TrCHInfo_setseq_0
. . . . . . (IntegerType)trchid = 1
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 144
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . (IntegerType)rateMatchingAttribute = 155
. . . . . . . . (CRC_Size)crc_Size = 3
. . . . . TrCHInfo_setseq_0
. . . . . . (IntegerType)trchid = 5
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 148
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . (IntegerType)rateMatchingAttribute = 170
. . . . . . . . (CRC_Size)crc_Size = 3
. . . . TFCS
. . . . . ExplicitTFCS_Configuration
. . . . . . TFCS_ReconfAdd
. . . . . . . ctfcSize
. . . . . . . . ctfc4Bit
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 0
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 1
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 2
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 3
. . . . . . . . . . PowerOffsetInformation
. . . . dlconnectedTrCHList
. . . . TFCS
. . . TrCH_LogCHMappingList1
. . . . ulconnectedTrCHList
. . . . . TrCH_LogCHMappingList1_setseq_0
. . . . . . (IntegerType)trchid = 1
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 7
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 5
. . . . . . . . (IntegerType)rB_Identity = -12
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . TrCH_LogCHMappingList1_setseq_0
. . . . . . (IntegerType)trchid = 5
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . (IntegerType)rB_Identity = 1
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . (IntegerType)rB_Identity = 2
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . (IntegerType)rB_Identity = 3
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . (IntegerType)rB_Identity = 4
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . dlconnectedTrCHList
- Constraint:
ca_CMAC_ReconfigInfo
- BinaryMessage:
30 81 e6 02 01 ff 02 01 14 0a 01 00 30 81 da 02 02 00 80 30 00 30 61 30 46 30 21 02 01 01 30 1c 30 0e 30 0c 02 02 00 90 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 9b 0a 01 03 30 21 02 01 05 30 1c 30 0e 30 0c 02 02 00 94 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 aa 0a 01 03 30 17 30 30 14 30 03 02 01 00 30 03 02 01 01 30 03 02 01 02 30 03 02 01 03 30 6f 30 6d 30 18 02 01 01 30 13 30 11 30 0c 0a 01 00 0a 01 00 02 01 07 0a 01 05 02 01 f4 30 51 02 01 05 30 4c 30 11 30 0c 0a 01 00 0a 01 00 02 01 01 0a 01 04 02 01 01 30 11 30 0c 0a 01 00 0a 01 00 02 01 02 0a 01 04 02 01 02 30 11 30 0c 0a 01 00 0a 01 00 02 01 03 0a 01 04 02 01 03 30 11 30 0c 0a 01 00 0a 01 00 02 01 04 0a 01 04 02 01 04

- No.: 2748
- Timestamp: 20:44:23:884_0
- RFN: 4829
- Chip: 17152
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_SS_2DCH_Modify LINE 14
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 14

- No.: 2751
- Timestamp: 20:44:23:895_0
- RFN: 4830
- Chip: 20736
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB_TM_Cfg_RLC LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = -12
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_TM_RLC_Mode
. . . . . . (BooleanType)segmentationIndication = TRUE
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 144
. . . . . UL_RLC_Mode
. . . . . . UL_TM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . (BooleanType)segmentationIndication = TRUE
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = 7
. . . . (IntegerType)dLlogicalChannelIdentity = 7
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_TM_Info
- BinaryMessage:
30 25 02 01 ff 02 01 f4 0a 01 00 30 1a 30 10 30 03 01 01 ff 30 09 02 02 00 90 30 03 01 01 ff 30 06 02 01 07 02 01 07

- No.: 2755
- Timestamp: 20:44:23:909_0
- RFN: 4832
- Chip: 512
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB_TM_Cfg_RLC LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = -12
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 f4

- No.: 2763
- Timestamp: 20:44:23:918_1
- RFN: 4832
- Chip: 33280
- Event: Start Timer
- Source: ts_RRC_ReceiveRB_SetupCmpl LINE 2
- Message Structure:
no details available
- Constraint:
t_WaitMS (13500 Ms)
- BinaryMessage:

- No.: 2772
- Timestamp: 20:44:25:619_0
- RFN: 5002
- Chip: 35072
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_IND
- Source: ts_RRC_ReceiveRB_SetupCmpl:lt_CipheringNotStartedAM_RAB LINE 4
- Message Structure:
RLC_AM_DATA_IND
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. IntegrityResult
. . (IntegrityStatus)integrityUsed = 0
. aM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "11011110110000110001011001100110"
. . . . (IntegerType)rrc_MessageSequenceNumber = 4
. . . UL_DCCH_MessageType
. . . . RadioBearerSetupComplete
. . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . IntegrityProtActivationInfo
. . . . . (IntegerType)ul_TimingAdvance = 0
. . . . . (BitStringType)start_Value[20] = "00000000000000000100"
. . . . . (IntegerType)count_C_ActivationTime = 0
. . . . . UL_CounterSynchronisationInfo
. . . . . laterNonCriticalExtensions
. . . . . . (BitStringType)radioBearerSetupComplete_r3_add_ext = 0
. . . . . . nonCriticalExtensions
- Constraint:
car_RB_SetUpCmpl
- BinaryMessage:
30 12 02 01 ff 02 01 02 0a 01 00 ef 61 8b 33 23 c8 00 00 08

- No.: 2773
- Timestamp: 20:44:25:620_0
- RFN: 5003
- Chip: 2048
- Event: Cancel Timer
- Source: ts_RRC_ReceiveRB_SetupCmpl:lt_CipheringNotStartedAM_RAB LINE 4
- Message Structure:
no details available
- Constraint:
t_WaitMS
- BinaryMessage:

- No.: 2774
- Timestamp: 20:44:25:621_0
- RFN: 5003
- Chip: 3072
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ReceiveRB_SetupCmpl:lt_CipheringNotStartedAM_RAB LINE 4
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2799
- Timestamp: 20:44:25:658_0
- RFN: 5006
- Chip: 30720
- Event: Send
- PCO: Dc
- Message: RRC_DataReq
- Source: ts_TC_CloseUE_TestLoop LINE 6
- Message Structure:
RRC_DataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[-1] = -
. (SapId)sapId[1] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. CLOSEUETESTLOOP
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)tCProtocolDiscriminator[4] = '1111'B
. . (MsgType)msgType[8] = '01000000'B
. . (UE_TestLoopMode)uE_TestLoopMode[1] = '00'O
. . UE_TestLoopMode1LB_Setup
. . . (Length)iel[1] = '03'O
. . . LB_SetupRB_IE
. . . . (BitStringType)rLC_SDU_Size[16] = '0000000001111000'B
. . . . (BitStringType)spare_2[3] = '000'B
. . . . (BitStringType)rB_Identity[5] = '10100'B
. . . LB_SetupRB_IE
. . . LB_SetupRB_IE
. . . LB_SetupRB_IE
- Constraint:
ca_PS_DataReq
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 0f 40 00 03 00 78 14

- No.: 2800
- Timestamp: 20:44:25:659_0
- RFN: 5006
- Chip: 35840
- Event: Start Timer
- Source: ts_TC_CloseUE_TestLoop LINE 6
- Message Structure:
no details available
- Constraint:
t_Dly (5000 Ms)
- BinaryMessage:

- No.: 2804
- Timestamp: 20:44:25:933_0
- RFN: 5034
- Chip: 12288
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_TC_CloseUE_TestLoop LINE 7
- Message Structure:
RRC_DataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. (START_Value)start[0] = -
. CLOSEUETESTLOOPCOMPLETE
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)tCProtocolDiscriminator[4] = '1111'B
. . (MsgType)msgType[8] = '01000001'B
- Constraint:
car_PS_UplinkDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 0f 41

- No.: 2805
- Timestamp: 20:44:25:934_0
- RFN: 5034
- Chip: 15616
- Event: Cancel Timer
- Source: ts_TC_CloseUE_TestLoop LINE 7
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 2806
- Timestamp: 20:44:25:934_1
- RFN: 5034
- Chip: 16384
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_TC_CloseUE_TestLoop LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2819
- Timestamp: 20:44:25:957_1
- RFN: 5036
- Chip: 29184
- Event: Start Timer
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 6
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 2826
- Timestamp: 20:44:25:981_1
- RFN: 5039
- Chip: 4608
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 2850
- Timestamp: 20:44:26:026_0
- RFN: 5043
- Chip: 25600
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000000'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'FFE665A5C5CA3452085408ABEECE4B'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 01 1e ff e6 65 a5 c5 ca 34 52 08 54 08 ab ee ce 4b

- No.: 2859
- Timestamp: 20:44:26:039_1
- RFN: 5044
- Chip: 37888
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 2860
- Timestamp: 20:44:26:040_0
- RFN: 5045
- Chip: 256
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2865
- Timestamp: 20:44:26:060_1
- RFN: 5047
- Chip: 1536
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 2889
- Timestamp: 20:44:26:104_0
- RFN: 5051
- Chip: 18944
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000001'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '0B813FD337873F2CD1E29AE91BD6C8'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 09 1e 0b 81 3f d3 37 87 3f 2c d1 e2 9a e9 1b d6 c8

- No.: 2898
- Timestamp: 20:44:26:118_0
- RFN: 5052
- Chip: 32768
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 2899
- Timestamp: 20:44:26:118_1
- RFN: 5052
- Chip: 33536
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2904
- Timestamp: 20:44:26:138_0
- RFN: 5054
- Chip: 33024
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 2928
- Timestamp: 20:44:26:186_0
- RFN: 5059
- Chip: 24064
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000010'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'E14FDE630F8195688EBE465F09816A'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 11 1e e1 4f de 63 0f 81 95 68 8e be 46 5f 09 81 6a

- No.: 2937
- Timestamp: 20:44:26:199_1
- RFN: 5060
- Chip: 36352
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 2938
- Timestamp: 20:44:26:200_0
- RFN: 5060
- Chip: 37376
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2941
- Timestamp: 20:44:26:207_0
- RFN: 5061
- Chip: 26112
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000000'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = 'FFE665A5C5CA3452085408ABEECE4B'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 05 1e ff e6 65 a5 c5 ca 34 52 08 54 08 ab ee ce 4b

- No.: 2958
- Timestamp: 20:44:26:233_0
- RFN: 5064
- Chip: 10496
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2961
- Timestamp: 20:44:26:236_1
- RFN: 5064
- Chip: 23552
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 2985
- Timestamp: 20:44:26:284_0
- RFN: 5069
- Chip: 16640
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000011'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '8EEB1B83953DD362DAE3B06D5B76D8'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 19 1e 8e eb 1b 83 95 3d d3 62 da e3 b0 6d 5b 76 d8

- No.: 2994
- Timestamp: 20:44:26:297_1
- RFN: 5070
- Chip: 28416
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 2995
- Timestamp: 20:44:26:297_2
- RFN: 5070
- Chip: 29440
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2998
- Timestamp: 20:44:26:305_0
- RFN: 5071
- Chip: 18944
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000001'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '0B813FD337873F2CD1E29AE91BD6C8'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 0d 1e 0b 81 3f d3 37 87 3f 2c d1 e2 9a e9 1b d6 c8

- No.: 3015
- Timestamp: 20:44:26:333_1
- RFN: 5074
- Chip: 12544
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3018
- Timestamp: 20:44:26:340_0
- RFN: 5075
- Chip: 2048
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000010'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = 'E14FDE630F8195688EBE465F09816A'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 15 1e e1 4f de 63 0f 81 95 68 8e be 46 5f 09 81 6a

- No.: 3035
- Timestamp: 20:44:26:366_0
- RFN: 5077
- Chip: 23808
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3038
- Timestamp: 20:44:26:369_0
- RFN: 5077
- Chip: 36608
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 3062
- Timestamp: 20:44:26:414_0
- RFN: 5082
- Chip: 17152
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000100'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'E3E53087EA645A09017FD99C3CACBB'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 21 1e e3 e5 30 87 ea 64 5a 09 01 7f d9 9c 3c ac bb

- No.: 3071
- Timestamp: 20:44:26:429_1
- RFN: 5083
- Chip: 38144
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 3072
- Timestamp: 20:44:26:429_2
- RFN: 5084
- Chip: 512
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3075
- Timestamp: 20:44:26:437_0
- RFN: 5084
- Chip: 29184
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000011'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '8EEB1B83953DD362DAE3B06D5B76D8'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 1d 1e 8e eb 1b 83 95 3d d3 62 da e3 b0 6d 5b 76 d8

- No.: 3092
- Timestamp: 20:44:26:463_2
- RFN: 5087
- Chip: 15360
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3095
- Timestamp: 20:44:26:466_1
- RFN: 5087
- Chip: 28416
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 3119
- Timestamp: 20:44:26:513_0
- RFN: 5092
- Chip: 11264
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000101'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '46DF1CD61DA9C435F89943DF9CC34A'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 29 1e 46 df 1c d6 1d a9 c4 35 f8 99 43 df 9c c3 4a

- No.: 3128
- Timestamp: 20:44:26:526_0
- RFN: 5093
- Chip: 23552
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 3129
- Timestamp: 20:44:26:526_1
- RFN: 5093
- Chip: 24576
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3134
- Timestamp: 20:44:26:551_1
- RFN: 5096
- Chip: 4096
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 3158
- Timestamp: 20:44:26:598_0
- RFN: 5100
- Chip: 33024
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000110'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'DEE31AD6E24FA1903D53778D949742'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 31 1e de e3 1a d6 e2 4f a1 90 3d 53 77 8d 94 97 42

- No.: 3167
- Timestamp: 20:44:26:612_0
- RFN: 5102
- Chip: 7424
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 3168
- Timestamp: 20:44:26:612_1
- RFN: 5102
- Chip: 8192
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3171
- Timestamp: 20:44:26:619_0
- RFN: 5102
- Chip: 35584
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000100'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = 'E3E53087EA645A09017FD99C3CACBB'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 25 1e e3 e5 30 87 ea 64 5a 09 01 7f d9 9c 3c ac bb

- No.: 3188
- Timestamp: 20:44:26:645_0
- RFN: 5105
- Chip: 19456
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3191
- Timestamp: 20:44:26:648_1
- RFN: 5105
- Chip: 32768
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 3215
- Timestamp: 20:44:26:695_0
- RFN: 5110
- Chip: 23552
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000111'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '750DD49DE9CE9E430AD448A14575D8'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 39 1e 75 0d d4 9d e9 ce 9e 43 0a d4 48 a1 45 75 d8

- No.: 3224
- Timestamp: 20:44:26:709_0
- RFN: 5111
- Chip: 36864
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 3225
- Timestamp: 20:44:26:709_1
- RFN: 5111
- Chip: 37888
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3228
- Timestamp: 20:44:26:716_0
- RFN: 5112
- Chip: 27648
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000101'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '46DF1CD61DA9C435F89943DF9CC34A'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 2d 1e 46 df 1c d6 1d a9 c4 35 f8 99 43 df 9c c3 4a

- No.: 3245
- Timestamp: 20:44:26:742_3
- RFN: 5115
- Chip: 11776
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3248
- Timestamp: 20:44:26:748_1
- RFN: 5115
- Chip: 33536
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 3272
- Timestamp: 20:44:26:795_0
- RFN: 5120
- Chip: 20480
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000001000'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '9C160255088140200555DDC9CBCB9E'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 41 1e 9c 16 02 55 08 81 40 20 05 55 dd c9 cb cb 9e

- No.: 3281
- Timestamp: 20:44:26:809_0
- RFN: 5121
- Chip: 33280
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 3282
- Timestamp: 20:44:26:809_1
- RFN: 5121
- Chip: 34304
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3285
- Timestamp: 20:44:26:816_0
- RFN: 5122
- Chip: 23808
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000110'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = 'DEE31AD6E24FA1903D53778D949742'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 35 1e de e3 1a d6 e2 4f a1 90 3d 53 77 8d 94 97 42

- No.: 3302
- Timestamp: 20:44:26:842_1
- RFN: 5125
- Chip: 7680
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3305
- Timestamp: 20:44:26:845_1
- RFN: 5125
- Chip: 29696
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 3329
- Timestamp: 20:44:26:893_0
- RFN: 5130
- Chip: 13568
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000001001'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'C31F833F866A5BA390680EAB11282E'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 49 1e c3 1f 83 3f 86 6a 5b a3 90 68 0e ab 11 28 2e

- No.: 3338
- Timestamp: 20:44:26:906_1
- RFN: 5131
- Chip: 25856
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 3339
- Timestamp: 20:44:26:907_0
- RFN: 5131
- Chip: 26880
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3342
- Timestamp: 20:44:26:914_0
- RFN: 5132
- Chip: 16640
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000111'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '750DD49DE9CE9E430AD448A14575D8'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 3d 1e 75 0d d4 9d e9 ce 9e 43 0a d4 48 a1 45 75 d8

- No.: 3359
- Timestamp: 20:44:26:940_1
- RFN: 5135
- Chip: 768
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3362
- Timestamp: 20:44:26:943_1
- RFN: 5135
- Chip: 14592
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 3386
- Timestamp: 20:44:26:991_0
- RFN: 5140
- Chip: 4864
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000001010'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'AE44F5E7658F6B247A0C54A21057F7'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 51 1e ae 44 f5 e7 65 8f 6b 24 7a 0c 54 a2 10 57 f7

- No.: 3395
- Timestamp: 20:44:27:005_0
- RFN: 5141
- Chip: 19968
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 3396
- Timestamp: 20:44:27:005_1
- RFN: 5141
- Chip: 20992
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3399
- Timestamp: 20:44:27:012_0
- RFN: 5142
- Chip: 11776
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000001000'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '9C160255088140200555DDC9CBCB9E'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 45 1e 9c 16 02 55 08 81 40 20 05 55 dd c9 cb cb 9e

- No.: 3416
- Timestamp: 20:44:27:038_3
- RFN: 5144
- Chip: 34304
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3419
- Timestamp: 20:44:27:042_0
- RFN: 5145
- Chip: 9472
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 3443
- Timestamp: 20:44:27:090_0
- RFN: 5150
- Chip: 2560
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000001011'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '3278595C235077F267A59097E8CEB4'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 59 1e 32 78 59 5c 23 50 77 f2 67 a5 90 97 e8 ce b4

- No.: 3452
- Timestamp: 20:44:27:103_1
- RFN: 5151
- Chip: 16128
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 3453
- Timestamp: 20:44:27:103_2
- RFN: 5151
- Chip: 16896
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3456
- Timestamp: 20:44:27:111_0
- RFN: 5152
- Chip: 5888
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000001001'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = 'C31F833F866A5BA390680EAB11282E'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 4d 1e c3 1f 83 3f 86 6a 5b a3 90 68 0e ab 11 28 2e

- No.: 3473
- Timestamp: 20:44:27:137_3
- RFN: 5154
- Chip: 28160
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3476
- Timestamp: 20:44:27:141_0
- RFN: 5155
- Chip: 2560
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 3500
- Timestamp: 20:44:27:189_0
- RFN: 5159
- Chip: 34048
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000001100'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'EDE49A16FDB36D2485EA3107D59DC3'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 61 1e ed e4 9a 16 fd b3 6d 24 85 ea 31 07 d5 9d c3

- No.: 3509
- Timestamp: 20:44:27:202_0
- RFN: 5161
- Chip: 8192
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 3510
- Timestamp: 20:44:27:202_1
- RFN: 5161
- Chip: 8960
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3513
- Timestamp: 20:44:27:209_0
- RFN: 5161
- Chip: 36608
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000001010'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = 'AE44F5E7658F6B247A0C54A21057F7'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 55 1e ae 44 f5 e7 65 8f 6b 24 7a 0c 54 a2 10 57 f7

- No.: 3530
- Timestamp: 20:44:27:235_2
- RFN: 5164
- Chip: 20992
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3533
- Timestamp: 20:44:27:238_1
- RFN: 5164
- Chip: 33792
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 3557
- Timestamp: 20:44:27:283_0
- RFN: 5169
- Chip: 14080
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000001101'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '60700D5488BEB9B96C24AF44DF498B'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 69 1e 60 70 0d 54 88 be b9 b9 6c 24 af 44 df 49 8b

- No.: 3566
- Timestamp: 20:44:27:295_0
- RFN: 5170
- Chip: 20480
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 3567
- Timestamp: 20:44:27:295_1
- RFN: 5170
- Chip: 21248
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3570
- Timestamp: 20:44:27:301_0
- RFN: 5171
- Chip: 6656
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000001011'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '3278595C235077F267A59097E8CEB4'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 5d 1e 32 78 59 5c 23 50 77 f2 67 a5 90 97 e8 ce b4

- No.: 3587
- Timestamp: 20:44:27:327_2
- RFN: 5173
- Chip: 29696
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3590
- Timestamp: 20:44:27:332_1
- RFN: 5174
- Chip: 11264
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 3614
- Timestamp: 20:44:27:378_0
- RFN: 5178
- Chip: 32768
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000001110'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'C135788C14A8BBEC64A5EF64DA1C56'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 71 1e c1 35 78 8c 14 a8 bb ec 64 a5 ef 64 da 1c 56

- No.: 3623
- Timestamp: 20:44:27:391_0
- RFN: 5180
- Chip: 6912
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 3624
- Timestamp: 20:44:27:391_1
- RFN: 5180
- Chip: 7680
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3627
- Timestamp: 20:44:27:398_0
- RFN: 5180
- Chip: 35328
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000001100'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = 'EDE49A16FDB36D2485EA3107D59DC3'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 65 1e ed e4 9a 16 fd b3 6d 24 85 ea 31 07 d5 9d c3

- No.: 3644
- Timestamp: 20:44:27:425_3
- RFN: 5183
- Chip: 20224
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3647
- Timestamp: 20:44:27:435_0
- RFN: 5184
- Chip: 18688
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000001101'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '60700D5488BEB9B96C24AF44DF498B'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 6d 1e 60 70 0d 54 88 be b9 b9 6c 24 af 44 df 49 8b

- No.: 3664
- Timestamp: 20:44:27:461_1
- RFN: 5187
- Chip: 3328
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3667
- Timestamp: 20:44:27:464_1
- RFN: 5187
- Chip: 16640
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 3691
- Timestamp: 20:44:27:509_0
- RFN: 5191
- Chip: 37120
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000001111'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '08FEB312D7B738D3E2CFB4C74A7458'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 79 1e 08 fe b3 12 d7 b7 38 d3 e2 cf b4 c7 4a 74 58

- No.: 3700
- Timestamp: 20:44:27:523_0
- RFN: 5193
- Chip: 11264
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 3701
- Timestamp: 20:44:27:523_1
- RFN: 5193
- Chip: 12032
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3706
- Timestamp: 20:44:27:536_0
- RFN: 5194
- Chip: 22528
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000001110'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = 'C135788C14A8BBEC64A5EF64DA1C56'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 75 1e c1 35 78 8c 14 a8 bb ec 64 a5 ef 64 da 1c 56

- No.: 3723
- Timestamp: 20:44:27:562_0
- RFN: 5197
- Chip: 7424
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3726
- Timestamp: 20:44:27:565_1
- RFN: 5197
- Chip: 20736
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 3750
- Timestamp: 20:44:27:610_0
- RFN: 5202
- Chip: 2048
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000010000'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'A3EF9B3C79F3CD348740DFE330780C'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 81 1e a3 ef 9b 3c 79 f3 cd 34 87 40 df e3 30 78 0c

- No.: 3759
- Timestamp: 20:44:27:623_1
- RFN: 5203
- Chip: 14848
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 3760
- Timestamp: 20:44:27:624_0
- RFN: 5203
- Chip: 15872
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3765
- Timestamp: 20:44:27:654_0
- RFN: 5206
- Chip: 18688
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000001111'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '08FEB312D7B738D3E2CFB4C74A7458'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 7d 1e 08 fe b3 12 d7 b7 38 d3 e2 cf b4 c7 4a 74 58

- No.: 3782
- Timestamp: 20:44:27:680_0
- RFN: 5209
- Chip: 1536
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3785
- Timestamp: 20:44:27:683_1
- RFN: 5209
- Chip: 15616
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 3809
- Timestamp: 20:44:27:728_0
- RFN: 5213
- Chip: 34560
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000010001'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '01FFCCCB4B8B9468A410A81157DD9C'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 89 1e 01 ff cc cb 4b 8b 94 68 a4 10 a8 11 57 dd 9c

- No.: 3818
- Timestamp: 20:44:27:743_0
- RFN: 5215
- Chip: 9472
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 3819
- Timestamp: 20:44:27:743_1
- RFN: 5215
- Chip: 10496
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3824
- Timestamp: 20:44:27:761_1
- RFN: 5217
- Chip: 3584
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 3848
- Timestamp: 20:44:27:809_0
- RFN: 5221
- Chip: 34816
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000010010'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '9617027FA66F0E7E59A3C535D237AD'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 91 1e 96 17 02 7f a6 6f 0e 7e 59 a3 c5 35 d2 37 ad

- No.: 3857
- Timestamp: 20:44:27:822_1
- RFN: 5223
- Chip: 8960
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 3858
- Timestamp: 20:44:27:822_2
- RFN: 5223
- Chip: 9728
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3861
- Timestamp: 20:44:27:829_0
- RFN: 5223
- Chip: 36864
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000010000'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = 'A3EF9B3C79F3CD348740DFE330780C'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 85 1e a3 ef 9b 3c 79 f3 cd 34 87 40 df e3 30 78 0c

- No.: 3878
- Timestamp: 20:44:27:856_1
- RFN: 5226
- Chip: 24064
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3881
- Timestamp: 20:44:27:859_1
- RFN: 5226
- Chip: 37120
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 3905
- Timestamp: 20:44:27:907_0
- RFN: 5231
- Chip: 29440
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000010011'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '91C29FBCC61F032AD11D7C8CBE1302'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 99 1e 91 c2 9f bc c6 1f 03 2a d1 1d 7c 8c be 13 02

- No.: 3914
- Timestamp: 20:44:27:920_1
- RFN: 5233
- Chip: 3072
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 3915
- Timestamp: 20:44:27:920_2
- RFN: 5233
- Chip: 4096
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3918
- Timestamp: 20:44:27:928_0
- RFN: 5233
- Chip: 31744
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000010001'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '01FFCCCB4B8B9468A410A81157DD9C'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 8d 1e 01 ff cc cb 4b 8b 94 68 a4 10 a8 11 57 dd 9c

- No.: 3935
- Timestamp: 20:44:27:956_1
- RFN: 5236
- Chip: 25088
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3938
- Timestamp: 20:44:27:963_0
- RFN: 5237
- Chip: 14080
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000010010'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '9617027FA66F0E7E59A3C535D237AD'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 95 1e 96 17 02 7f a6 6f 0e 7e 59 a3 c5 35 d2 37 ad

- No.: 3955
- Timestamp: 20:44:27:989_2
- RFN: 5239
- Chip: 37376
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3958
- Timestamp: 20:44:27:992_1
- RFN: 5240
- Chip: 12032
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 3982
- Timestamp: 20:44:28:039_0
- RFN: 5245
- Chip: 0
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000010100'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'D51DD637072A7BA6C5B5C760DAB6ED'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 a1 1e d5 1d d6 37 07 2a 7b a6 c5 b5 c7 60 da b6 ed

- No.: 3991
- Timestamp: 20:44:28:056_1
- RFN: 5246
- Chip: 23808
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 3992
- Timestamp: 20:44:28:056_2
- RFN: 5246
- Chip: 24576
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3995
- Timestamp: 20:44:28:063_0
- RFN: 5247
- Chip: 13312
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000010011'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '91C29FBCC61F032AD11D7C8CBE1302'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 9d 1e 91 c2 9f bc c6 1f 03 2a d1 1d 7c 8c be 13 02

- No.: 4012
- Timestamp: 20:44:28:090_0
- RFN: 5249
- Chip: 36864
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4015
- Timestamp: 20:44:28:093_1
- RFN: 5250
- Chip: 11520
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 4039
- Timestamp: 20:44:28:138_0
- RFN: 5254
- Chip: 32256
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000010101'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'B1C7CA610FD4C8B41202FFB3387959'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 a9 1e b1 c7 ca 61 0f d4 c8 b4 12 02 ff b3 38 79 59

- No.: 4048
- Timestamp: 20:44:28:151_1
- RFN: 5256
- Chip: 6912
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 4049
- Timestamp: 20:44:28:152_0
- RFN: 5256
- Chip: 7936
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4054
- Timestamp: 20:44:28:180_1
- RFN: 5259
- Chip: 1280
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 4078
- Timestamp: 20:44:28:228_0
- RFN: 5263
- Chip: 31744
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000010110'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '768DBE39AC3B53886BF13287BF3986'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 b1 1e 76 8d be 39 ac 3b 53 88 6b f1 32 87 bf 39 86

- No.: 4087
- Timestamp: 20:44:28:241_0
- RFN: 5265
- Chip: 5888
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 4088
- Timestamp: 20:44:28:241_1
- RFN: 5265
- Chip: 6656
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4091
- Timestamp: 20:44:28:248_0
- RFN: 5265
- Chip: 34816
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000010100'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = 'D51DD637072A7BA6C5B5C760DAB6ED'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 a5 1e d5 1d d6 37 07 2a 7b a6 c5 b5 c7 60 da b6 ed

- No.: 4108
- Timestamp: 20:44:28:275_0
- RFN: 5268
- Chip: 20480
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4111
- Timestamp: 20:44:28:278_1
- RFN: 5268
- Chip: 33536
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 4135
- Timestamp: 20:44:28:325_0
- RFN: 5273
- Chip: 23296
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000010111'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '95BDC635ADC49F43207AA6EF1B292E'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 b9 1e 95 bd c6 35 ad c4 9f 43 20 7a a6 ef 1b 29 2e

- No.: 4144
- Timestamp: 20:44:28:339_0
- RFN: 5274
- Chip: 36608
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 4145
- Timestamp: 20:44:28:339_1
- RFN: 5274
- Chip: 37376
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4148
- Timestamp: 20:44:28:346_0
- RFN: 5275
- Chip: 27392
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000010101'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = 'B1C7CA610FD4C8B41202FFB3387959'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 ad 1e b1 c7 ca 61 0f d4 c8 b4 12 02 ff b3 38 79 59

- No.: 4165
- Timestamp: 20:44:28:375_3
- RFN: 5278
- Chip: 19968
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4168
- Timestamp: 20:44:28:382_0
- RFN: 5279
- Chip: 9216
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000010110'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '768DBE39AC3B53886BF13287BF3986'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 b5 1e 76 8d be 39 ac 3b 53 88 6b f1 32 87 bf 39 86

- No.: 4185
- Timestamp: 20:44:28:408_1
- RFN: 5281
- Chip: 30464
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4188
- Timestamp: 20:44:28:411_1
- RFN: 5282
- Chip: 5632
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 4212
- Timestamp: 20:44:28:457_0
- RFN: 5286
- Chip: 28928
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000011000'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '84EA1BA93BD39D3C8615A891428AEB'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 c1 1e 84 ea 1b a9 3b d3 9d 3c 86 15 a8 91 42 8a eb

- No.: 4221
- Timestamp: 20:44:28:470_1
- RFN: 5288
- Chip: 2816
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 4222
- Timestamp: 20:44:28:471_0
- RFN: 5288
- Chip: 3584
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4227
- Timestamp: 20:44:28:495_0
- RFN: 5290
- Chip: 19968
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000010111'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '95BDC635ADC49F43207AA6EF1B292E'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 bd 1e 95 bd c6 35 ad c4 9f 43 20 7a a6 ef 1b 29 2e

- No.: 4244
- Timestamp: 20:44:28:520_3
- RFN: 5293
- Chip: 3072
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4247
- Timestamp: 20:44:28:524_0
- RFN: 5293
- Chip: 16128
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 4271
- Timestamp: 20:44:28:569_0
- RFN: 5298
- Chip: 256
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000011001'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'B1382C04AA110280400AABBB939797'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 c9 1e b1 38 2c 04 aa 11 02 80 40 0a ab bb 93 97 97

- No.: 4280
- Timestamp: 20:44:28:583_0
- RFN: 5299
- Chip: 12288
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 4281
- Timestamp: 20:44:28:583_1
- RFN: 5299
- Chip: 13312
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4286
- Timestamp: 20:44:28:597_1
- RFN: 5300
- Chip: 28928
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 4310
- Timestamp: 20:44:28:644_0
- RFN: 5305
- Chip: 20480
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000011010'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '3D863F067F0CD4B74720D01D562250'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 d1 1e 3d 86 3f 06 7f 0c d4 b7 47 20 d0 1d 56 22 50

- No.: 4319
- Timestamp: 20:44:28:658_0
- RFN: 5306
- Chip: 33792
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 4320
- Timestamp: 20:44:28:658_1
- RFN: 5306
- Chip: 34560
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4323
- Timestamp: 20:44:28:665_0
- RFN: 5307
- Chip: 23808
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000011000'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '84EA1BA93BD39D3C8615A891428AEB'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 c5 1e 84 ea 1b a9 3b d3 9d 3c 86 15 a8 91 42 8a eb

- No.: 4340
- Timestamp: 20:44:28:692_3
- RFN: 5310
- Chip: 8960
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4343
- Timestamp: 20:44:28:696_1
- RFN: 5310
- Chip: 22272
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 4367
- Timestamp: 20:44:28:744_0
- RFN: 5315
- Chip: 14080
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000011011'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '5D5C89EBCECB1ED648F418A94420AF'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 d9 1e 5d 5c 89 eb ce cb 1e d6 48 f4 18 a9 44 20 af

- No.: 4376
- Timestamp: 20:44:28:757_0
- RFN: 5316
- Chip: 27392
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 4377
- Timestamp: 20:44:28:757_1
- RFN: 5316
- Chip: 28416
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4380
- Timestamp: 20:44:28:764_0
- RFN: 5317
- Chip: 17408
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000011001'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = 'B1382C04AA110280400AABBB939797'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 cd 1e b1 38 2c 04 aa 11 02 80 40 0a ab bb 93 97 97

- No.: 4397
- Timestamp: 20:44:28:793_3
- RFN: 5320
- Chip: 13824
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4400
- Timestamp: 20:44:28:801_0
- RFN: 5321
- Chip: 3328
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000011010'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '3D863F067F0CD4B74720D01D562250'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 d5 1e 3d 86 3f 06 7f 0c d4 b7 47 20 d0 1d 56 22 50

- No.: 4417
- Timestamp: 20:44:28:826_2
- RFN: 5323
- Chip: 25088
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4420
- Timestamp: 20:44:28:830_0
- RFN: 5324
- Chip: 0
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 4444
- Timestamp: 20:44:28:875_0
- RFN: 5328
- Chip: 21504
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000011100'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'EE64F0B2B846A0EFE4CF4B212FD19D'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 e1 1e ee 64 f0 b2 b8 46 a0 ef e4 cf 4b 21 2f d1 9d

- No.: 4453
- Timestamp: 20:44:28:891_0
- RFN: 5330
- Chip: 6144
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 4454
- Timestamp: 20:44:28:891_1
- RFN: 5330
- Chip: 6912
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4457
- Timestamp: 20:44:28:898_0
- RFN: 5330
- Chip: 34560
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000011011'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '5D5C89EBCECB1ED648F418A94420AF'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 dd 1e 5d 5c 89 eb ce cb 1e d6 48 f4 18 a9 44 20 af

- No.: 4474
- Timestamp: 20:44:28:924_3
- RFN: 5333
- Chip: 19456
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4477
- Timestamp: 20:44:28:928_0
- RFN: 5333
- Chip: 32768
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 4501
- Timestamp: 20:44:28:973_0
- RFN: 5338
- Chip: 13568
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000011101'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '69DBC9342DFB66DA490BD4620FAB3B'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 e9 1e 69 db c9 34 2d fb 66 da 49 0b d4 62 0f ab 3b

- No.: 4510
- Timestamp: 20:44:28:986_0
- RFN: 5339
- Chip: 27136
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 4511
- Timestamp: 20:44:28:986_1
- RFN: 5339
- Chip: 27904
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4516
- Timestamp: 20:44:29:004_1
- RFN: 5341
- Chip: 16128
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 4540
- Timestamp: 20:44:29:053_0
- RFN: 5346
- Chip: 10496
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000011110'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '86C0E01AA9117D7372D8495E89BE93'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 f1 1e 86 c0 e0 1a a9 11 7d 73 72 d8 49 5e 89 be 93

- No.: 4549
- Timestamp: 20:44:29:066_0
- RFN: 5347
- Chip: 23296
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 4550
- Timestamp: 20:44:29:066_1
- RFN: 5347
- Chip: 24576
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4553
- Timestamp: 20:44:29:073_0
- RFN: 5348
- Chip: 13568
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000011100'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = 'EE64F0B2B846A0EFE4CF4B212FD19D'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 e5 1e ee 64 f0 b2 b8 46 a0 ef e4 cf 4b 21 2f d1 9d

- No.: 4570
- Timestamp: 20:44:29:099_2
- RFN: 5350
- Chip: 36352
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4573
- Timestamp: 20:44:29:103_0
- RFN: 5351
- Chip: 11008
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 4597
- Timestamp: 20:44:29:150_0
- RFN: 5356
- Chip: 2816
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000011111'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '17826AF118295177D8C94BDEC9B438'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 f9 1e 17 82 6a f1 18 29 51 77 d8 c9 4b de c9 b4 38

- No.: 4606
- Timestamp: 20:44:29:164_0
- RFN: 5357
- Chip: 15616
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 4607
- Timestamp: 20:44:29:164_1
- RFN: 5357
- Chip: 16640
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4610
- Timestamp: 20:44:29:171_0
- RFN: 5358
- Chip: 5888
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000011101'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '69DBC9342DFB66DA490BD4620FAB3B'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 ed 1e 69 db c9 34 2d fb 66 da 49 0b d4 62 0f ab 3b

- No.: 4627
- Timestamp: 20:44:29:197_1
- RFN: 5360
- Chip: 28416
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4630
- Timestamp: 20:44:29:200_1
- RFN: 5361
- Chip: 3584
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 4654
- Timestamp: 20:44:29:248_0
- RFN: 5365
- Chip: 34048
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000100000'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'AC11FD6625AF6E71A7C59F698E94E8'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 01 1e ac 11 fd 66 25 af 6e 71 a7 c5 9f 69 8e 94 e8

- No.: 4663
- Timestamp: 20:44:29:261_1
- RFN: 5367
- Chip: 8448
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 4664
- Timestamp: 20:44:29:262_0
- RFN: 5367
- Chip: 9472
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4667
- Timestamp: 20:44:29:269_0
- RFN: 5367
- Chip: 37120
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000011110'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '86C0E01AA9117D7372D8495E89BE93'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 f5 1e 86 c0 e0 1a a9 11 7d 73 72 d8 49 5e 89 be 93

- No.: 4684
- Timestamp: 20:44:29:295_1
- RFN: 5370
- Chip: 22528
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4687
- Timestamp: 20:44:29:298_1
- RFN: 5370
- Chip: 35840
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 4711
- Timestamp: 20:44:29:347_0
- RFN: 5375
- Chip: 26880
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000100001'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'B147DF3678F3E79A690E81BFC660F0'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 09 1e b1 47 df 36 78 f3 e7 9a 69 0e 81 bf c6 60 f0

- No.: 4720
- Timestamp: 20:44:29:360_1
- RFN: 5377
- Chip: 2048
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 4721
- Timestamp: 20:44:29:361_0
- RFN: 5377
- Chip: 3072
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4724
- Timestamp: 20:44:29:368_0
- RFN: 5377
- Chip: 30464
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000011111'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '17826AF118295177D8C94BDEC9B438'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 fd 1e 17 82 6a f1 18 29 51 77 d8 c9 4b de c9 b4 38

- No.: 4741
- Timestamp: 20:44:29:396_3
- RFN: 5380
- Chip: 25088
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4744
- Timestamp: 20:44:29:404_0
- RFN: 5381
- Chip: 14592
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000100000'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = 'AC11FD6625AF6E71A7C59F698E94E8'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 05 1e ac 11 fd 66 25 af 6e 71 a7 c5 9f 69 8e 94 e8

- No.: 4761
- Timestamp: 20:44:29:429_3
- RFN: 5383
- Chip: 36864
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4764
- Timestamp: 20:44:29:433_0
- RFN: 5384
- Chip: 12032
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 4788
- Timestamp: 20:44:29:478_0
- RFN: 5388
- Chip: 32768
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000100010'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '1803FF9996971728D148215022AFBB'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 11 1e 18 03 ff 99 96 97 17 28 d1 48 21 50 22 af bb

- No.: 4797
- Timestamp: 20:44:29:494_0
- RFN: 5390
- Chip: 17408
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 4798
- Timestamp: 20:44:29:494_1
- RFN: 5390
- Chip: 18176
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4801
- Timestamp: 20:44:29:501_0
- RFN: 5391
- Chip: 7424
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000100001'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = 'B147DF3678F3E79A690E81BFC660F0'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 0d 1e b1 47 df 36 78 f3 e7 9a 69 0e 81 bf c6 60 f0

- No.: 4818
- Timestamp: 20:44:29:527_3
- RFN: 5393
- Chip: 30464
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4821
- Timestamp: 20:44:29:531_0
- RFN: 5394
- Chip: 5376
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 4845
- Timestamp: 20:44:29:576_0
- RFN: 5398
- Chip: 25856
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000100011'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '392C2E04FF4CDE1CFCB3478A6BA46F'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 19 1e 39 2c 2e 04 ff 4c de 1c fc b3 47 8a 6b a4 6f

- No.: 4854
- Timestamp: 20:44:29:589_1
- RFN: 5400
- Chip: 1280
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 4855
- Timestamp: 20:44:29:590_0
- RFN: 5400
- Chip: 2304
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4860
- Timestamp: 20:44:29:610_1
- RFN: 5402
- Chip: 3584
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 4884
- Timestamp: 20:44:29:659_0
- RFN: 5406
- Chip: 35328
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000100100'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '5B23853F798C3E0655A23AF9197C26'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 21 1e 5b 23 85 3f 79 8c 3e 06 55 a2 3a f9 19 7c 26

- No.: 4893
- Timestamp: 20:44:29:673_0
- RFN: 5408
- Chip: 10496
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 4894
- Timestamp: 20:44:29:673_1
- RFN: 5408
- Chip: 11264
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4897
- Timestamp: 20:44:29:680_0
- RFN: 5409
- Chip: 2048
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000100010'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '1803FF9996971728D148215022AFBB'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 15 1e 18 03 ff 99 96 97 17 28 d1 48 21 50 22 af bb

- No.: 4914
- Timestamp: 20:44:29:707_0
- RFN: 5411
- Chip: 26368
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4917
- Timestamp: 20:44:29:710_1
- RFN: 5412
- Chip: 1792
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 4941
- Timestamp: 20:44:29:758_0
- RFN: 5416
- Chip: 33536
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000100101'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '05AA3BAC6E0E54F74D8B6B8EC1B56D'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 29 1e 05 aa 3b ac 6e 0e 54 f7 4d 8b 6b 8e c1 b5 6d

- No.: 4950
- Timestamp: 20:44:29:772_0
- RFN: 5418
- Chip: 8448
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 4951
- Timestamp: 20:44:29:772_1
- RFN: 5418
- Chip: 9216
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4954
- Timestamp: 20:44:29:779_0
- RFN: 5418
- Chip: 36608
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000100011'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '392C2E04FF4CDE1CFCB3478A6BA46F'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 1d 1e 39 2c 2e 04 ff 4c de 1c fc b3 47 8a 6b a4 6f

- No.: 4971
- Timestamp: 20:44:29:835_0
- RFN: 5424
- Chip: 20480
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4974
- Timestamp: 20:44:29:842_0
- RFN: 5425
- Chip: 9216
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000100100'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '5B23853F798C3E0655A23AF9197C26'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 25 1e 5b 23 85 3f 79 8c 3e 06 55 a2 3a f9 19 7c 26

- No.: 4991
- Timestamp: 20:44:29:942_3
- RFN: 5435
- Chip: 8704
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4994
- Timestamp: 20:44:29:950_0
- RFN: 5435
- Chip: 37888
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000100101'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '05AA3BAC6E0E54F74D8B6B8EC1B56D'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 2d 1e 05 aa 3b ac 6e 0e 54 f7 4d 8b 6b 8e c1 b5 6d

- No.: 5011
- Timestamp: 20:44:29:976_2
- RFN: 5438
- Chip: 23296
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 5014
- Timestamp: 20:44:29:980_0
- RFN: 5438
- Chip: 37120
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 5038
- Timestamp: 20:44:30:027_0
- RFN: 5443
- Chip: 28672
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000100110'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'DB638F94C21FA991682405FF6670F2'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 31 1e db 63 8f 94 c2 1f a9 91 68 24 05 ff 66 70 f2

- No.: 5047
- Timestamp: 20:44:30:041_0
- RFN: 5445
- Chip: 4096
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 5048
- Timestamp: 20:44:30:041_1
- RFN: 5445
- Chip: 4864
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 5053
- Timestamp: 20:44:30:058_1
- RFN: 5446
- Chip: 32256
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 5077
- Timestamp: 20:44:30:105_0
- RFN: 5451
- Chip: 22528
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000100111'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'B2ED1B7C735876A710D7E2650F7E73'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 39 1e b2 ed 1b 7c 73 58 76 a7 10 d7 e2 65 0f 7e 73

- No.: 5086
- Timestamp: 20:44:30:119_1
- RFN: 5452
- Chip: 36608
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 5087
- Timestamp: 20:44:30:119_2
- RFN: 5452
- Chip: 37632
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 5092
- Timestamp: 20:44:30:136_1
- RFN: 5454
- Chip: 25344
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 5116
- Timestamp: 20:44:30:185_0
- RFN: 5459
- Chip: 23296
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000101000'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '0D2B7B8C6B5B893E8640F54DDE3652'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 41 1e 0d 2b 7b 8c 6b 5b 89 3e 86 40 f5 4d de 36 52

- No.: 5125
- Timestamp: 20:44:30:199_1
- RFN: 5461
- Chip: 512
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 5126
- Timestamp: 20:44:30:200_0
- RFN: 5461
- Chip: 1792
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 5129
- Timestamp: 20:44:30:207_0
- RFN: 5461
- Chip: 30464
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000100110'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = 'DB638F94C21FA991682405FF6670F2'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 35 1e db 63 8f 94 c2 1f a9 91 68 24 05 ff 66 70 f2

- No.: 5146
- Timestamp: 20:44:30:234_1
- RFN: 5464
- Chip: 17920
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 5149
- Timestamp: 20:44:30:238_0
- RFN: 5464
- Chip: 32512
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 5173
- Timestamp: 20:44:30:288_0
- RFN: 5469
- Chip: 32256
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000101001'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '5D09D4375277A73A790C2B51228515'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 49 1e 5d 09 d4 37 52 77 a7 3a 79 0c 2b 51 22 85 15

- No.: 5182
- Timestamp: 20:44:30:303_1
- RFN: 5471
- Chip: 12800
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 5183
- Timestamp: 20:44:30:303_2
- RFN: 5471
- Chip: 13568
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 5186
- Timestamp: 20:44:30:311_0
- RFN: 5472
- Chip: 3584
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000100111'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = 'B2ED1B7C735876A710D7E2650F7E73'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 3d 1e b2 ed 1b 7c 73 58 76 a7 10 d7 e2 65 0f 7e 73

- No.: 5203
- Timestamp: 20:44:30:340_3
- RFN: 5475
- Chip: 2304
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 5206
- Timestamp: 20:44:30:348_0
- RFN: 5475
- Chip: 31232
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000101000'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '0D2B7B8C6B5B893E8640F54DDE3652'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 45 1e 0d 2b 7b 8c 6b 5b 89 3e 86 40 f5 4d de 36 52

- No.: 5223
- Timestamp: 20:44:30:374_3
- RFN: 5478
- Chip: 18176
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 5226
- Timestamp: 20:44:30:378_1
- RFN: 5478
- Chip: 32000
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 5250
- Timestamp: 20:44:30:426_0
- RFN: 5483
- Chip: 23552
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000101010'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'D7627058095422050080155777272F'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 51 1e d7 62 70 58 09 54 22 05 00 80 15 57 77 27 2f

- No.: 5259
- Timestamp: 20:44:30:439_1
- RFN: 5484
- Chip: 37632
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 5260
- Timestamp: 20:44:30:439_2
- RFN: 5485
- Chip: 256
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 5265
- Timestamp: 20:44:30:454_0
- RFN: 5486
- Chip: 19456
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000101001'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '5D09D4375277A73A790C2B51228515'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 4d 1e 5d 09 d4 37 52 77 a7 3a 79 0c 2b 51 22 85 15

- No.: 5282
- Timestamp: 20:44:30:482_1
- RFN: 5489
- Chip: 9728
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 5285
- Timestamp: 20:44:30:485_1
- RFN: 5489
- Chip: 23808
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 5309
- Timestamp: 20:44:30:533_0
- RFN: 5494
- Chip: 13312
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000101011'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '2E7B0C7E0CFE19A96E8E41A03AAC44'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 59 1e 2e 7b 0c 7e 0c fe 19 a9 6e 8e 41 a0 3a ac 44

- No.: 5318
- Timestamp: 20:44:30:546_1
- RFN: 5495
- Chip: 28160
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 5319
- Timestamp: 20:44:30:547_0
- RFN: 5495
- Chip: 29696
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 5324
- Timestamp: 20:44:30:565_1
- RFN: 5497
- Chip: 19456
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 5348
- Timestamp: 20:44:30:615_0
- RFN: 5502
- Chip: 18176
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000101100'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'A0BAB913D79D963DAC91E831528841'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 61 1e a0 ba b9 13 d7 9d 96 3d ac 91 e8 31 52 88 41

- No.: 5357
- Timestamp: 20:44:30:628_1
- RFN: 5503
- Chip: 33280
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 5358
- Timestamp: 20:44:30:629_0
- RFN: 5503
- Chip: 34048
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 5361
- Timestamp: 20:44:30:636_0
- RFN: 5504
- Chip: 23808
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000101010'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = 'D7627058095422050080155777272F'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 55 1e d7 62 70 58 09 54 22 05 00 80 15 57 77 27 2f

- No.: 5378
- Timestamp: 20:44:30:664_0
- RFN: 5507
- Chip: 14592
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 5381
- Timestamp: 20:44:30:667_1
- RFN: 5507
- Chip: 29184
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 5405
- Timestamp: 20:44:30:717_0
- RFN: 5512
- Chip: 30208
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000101101'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '5FDCC9E165708D41DFC99E96425FA3'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 69 1e 5f dc c9 e1 65 70 8d 41 df c9 9e 96 42 5f a3

- No.: 5414
- Timestamp: 20:44:30:731_1
- RFN: 5514
- Chip: 7424
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 5415
- Timestamp: 20:44:30:732_0
- RFN: 5514
- Chip: 8448
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 5418
- Timestamp: 20:44:30:739_0
- RFN: 5514
- Chip: 36864
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000101011'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '2E7B0C7E0CFE19A96E8E41A03AAC44'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 5d 1e 2e 7b 0c 7e 0c fe 19 a9 6e 8e 41 a0 3a ac 44

- No.: 5435
- Timestamp: 20:44:30:767_2
- RFN: 5517
- Chip: 29952
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 5438
- Timestamp: 20:44:30:771_0
- RFN: 5518
- Chip: 4608
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 5462
- Timestamp: 20:44:30:822_0
- RFN: 5523
- Chip: 12032
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000101110'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '3AD3B792685BF6CDB49217A8C41F56'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 71 1e 3a d3 b7 92 68 5b f6 cd b4 92 17 a8 c4 1f 56

- No.: 5471
- Timestamp: 20:44:30:836_1
- RFN: 5524
- Chip: 26880
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 5472
- Timestamp: 20:44:30:836_2
- RFN: 5524
- Chip: 27904
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 5475
- Timestamp: 20:44:30:844_0
- RFN: 5525
- Chip: 19712
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000101100'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = 'A0BAB913D79D963DAC91E831528841'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 65 1e a0 ba b9 13 d7 9d 96 3d ac 91 e8 31 52 88 41

- No.: 5492
- Timestamp: 20:44:30:875_2
- RFN: 5528
- Chip: 19200
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 5495
- Timestamp: 20:44:30:883_0
- RFN: 5529
- Chip: 10240
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000101101'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '5FDCC9E165708D41DFC99E96425FA3'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 6d 1e 5f dc c9 e1 65 70 8d 41 df c9 9e 96 42 5f a3

- No.: 5512
- Timestamp: 20:44:30:910_0
- RFN: 5531
- Chip: 37120
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 5515
- Timestamp: 20:44:30:913_1
- RFN: 5532
- Chip: 13312
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 5539
- Timestamp: 20:44:30:961_0
- RFN: 5537
- Chip: 3072
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000101111'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '770D81C0355222FAE6E5B092BD137D'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 79 1e 77 0d 81 c0 35 52 22 fa e6 e5 b0 92 bd 13 7d

- No.: 5548
- Timestamp: 20:44:30:977_1
- RFN: 5538
- Chip: 29440
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 5549
- Timestamp: 20:44:30:978_0
- RFN: 5538
- Chip: 30464
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 5552
- Timestamp: 20:44:30:985_0
- RFN: 5539
- Chip: 20992
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000101110'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '3AD3B792685BF6CDB49217A8C41F56'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 75 1e 3a d3 b7 92 68 5b f6 cd b4 92 17 a8 c4 1f 56

- No.: 5569
- Timestamp: 20:44:31:014_0
- RFN: 5542
- Chip: 15360
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 5572
- Timestamp: 20:44:31:017_1
- RFN: 5542
- Chip: 28928
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 5596
- Timestamp: 20:44:31:065_0
- RFN: 5547
- Chip: 19968
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000110000'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '262F04D5E23052A2EFB19297BD9368'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 81 1e 26 2f 04 d5 e2 30 52 a2 ef b1 92 97 bd 93 68

- No.: 5605
- Timestamp: 20:44:31:079_0
- RFN: 5548
- Chip: 35328
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 5606
- Timestamp: 20:44:31:079_1
- RFN: 5548
- Chip: 36096
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 5611
- Timestamp: 20:44:31:097_1
- RFN: 5550
- Chip: 30464
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 5635
- Timestamp: 20:44:31:147_0
- RFN: 5555
- Chip: 32256
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000110001'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '715823FACC4B5EDCE34F8B3ED31D29'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 89 1e 71 58 23 fa cc 4b 5e dc e3 4f 8b 3e d3 1d 29

- No.: 5644
- Timestamp: 20:44:31:161_1
- RFN: 5557
- Chip: 8704
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 5645
- Timestamp: 20:44:31:162_0
- RFN: 5557
- Chip: 9984
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 5648
- Timestamp: 20:44:31:169_0
- RFN: 5558
- Chip: 256
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000101111'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '770D81C0355222FAE6E5B092BD137D'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 7d 1e 77 0d 81 c0 35 52 22 fa e6 e5 b0 92 bd 13 7d

- No.: 5665
- Timestamp: 20:44:31:197_3
- RFN: 5560
- Chip: 27904
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 5668
- Timestamp: 20:44:31:201_1
- RFN: 5561
- Chip: 3328
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 5692
- Timestamp: 20:44:31:251_0
- RFN: 5566
- Chip: 5120
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000110010'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'D1628FBE6CF1E7CF34D21D037F8CC1'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 91 1e d1 62 8f be 6c f1 e7 cf 34 d2 1d 03 7f 8c c1

- No.: 5701
- Timestamp: 20:44:31:265_1
- RFN: 5567
- Chip: 21248
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 5702
- Timestamp: 20:44:31:266_0
- RFN: 5567
- Chip: 22272
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 5705
- Timestamp: 20:44:31:273_0
- RFN: 5568
- Chip: 13312
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000110000'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '262F04D5E23052A2EFB19297BD9368'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 85 1e 26 2f 04 d5 e2 30 52 a2 ef b1 92 97 bd 93 68

- No.: 5722
- Timestamp: 20:44:31:303_2
- RFN: 5571
- Chip: 13312
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 5725
- Timestamp: 20:44:31:311_0
- RFN: 5572
- Chip: 4352
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000110001'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '715823FACC4B5EDCE34F8B3ED31D29'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 8d 1e 71 58 23 fa cc 4b 5e dc e3 4f 8b 3e d3 1d 29

- No.: 5742
- Timestamp: 20:44:31:337_2
- RFN: 5574
- Chip: 29440
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 5745
- Timestamp: 20:44:31:341_1
- RFN: 5575
- Chip: 4864
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 5769
- Timestamp: 20:44:31:389_0
- RFN: 5579
- Chip: 37376
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000110011'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'E03007FF332D2E2E51A29042A0455F'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 99 1e e0 30 07 ff 33 2d 2e 2e 51 a2 90 42 a0 45 5f

- No.: 5778
- Timestamp: 20:44:31:403_0
- RFN: 5581
- Chip: 13312
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 5779
- Timestamp: 20:44:31:403_1
- RFN: 5581
- Chip: 14336
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 5784
- Timestamp: 20:44:31:417_0
- RFN: 5582
- Chip: 28928
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000110010'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = 'D1628FBE6CF1E7CF34D21D037F8CC1'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 95 1e d1 62 8f be 6c f1 e7 cf 34 d2 1d 03 7f 8c c1

- No.: 5801
- Timestamp: 20:44:31:444_2
- RFN: 5585
- Chip: 18944
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 5804
- Timestamp: 20:44:31:448_1
- RFN: 5585
- Chip: 33280
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 5828
- Timestamp: 20:44:31:496_0
- RFN: 5590
- Chip: 27648
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000110100'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '7672585C09FE99BC39F9668F14D748'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 a1 1e 76 72 58 5c 09 fe 99 bc 39 f9 66 8f 14 d7 48

- No.: 5837
- Timestamp: 20:44:31:511_1
- RFN: 5592
- Chip: 4352
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 5838
- Timestamp: 20:44:31:511_2
- RFN: 5592
- Chip: 5120
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 5843
- Timestamp: 20:44:31:535_0
- RFN: 5594
- Chip: 20480
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000110011'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = 'E03007FF332D2E2E51A29042A0455F'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 9d 1e e0 30 07 ff 33 2d 2e 2e 51 a2 90 42 a0 45 5f

- No.: 5860
- Timestamp: 20:44:31:562_3
- RFN: 5597
- Chip: 8704
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 5863
- Timestamp: 20:44:31:566_0
- RFN: 5597
- Chip: 22784
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 5887
- Timestamp: 20:44:31:613_0
- RFN: 5602
- Chip: 14336
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000110101'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'DEB6470A7EF3187C0CAB4475F232F8'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 a9 1e de b6 47 0a 7e f3 18 7c 0c ab 44 75 f2 32 f8

- No.: 5896
- Timestamp: 20:44:31:627_1
- RFN: 5603
- Chip: 29696
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 5897
- Timestamp: 20:44:31:628_0
- RFN: 5603
- Chip: 30720
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 5902
- Timestamp: 20:44:31:655_0
- RFN: 5606
- Chip: 20480
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000110100'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '7672585C09FE99BC39F9668F14D748'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 a5 1e 76 72 58 5c 09 fe 99 bc 39 f9 66 8f 14 d7 48

- No.: 5919
- Timestamp: 20:44:31:682_1
- RFN: 5609
- Chip: 9472
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 5922
- Timestamp: 20:44:31:686_0
- RFN: 5609
- Chip: 23552
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 5946
- Timestamp: 20:44:31:733_0
- RFN: 5614
- Chip: 15616
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000110110'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '4C0B547758DC1CA9EE9B16D71D836A'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 b1 1e 4c 0b 54 77 58 dc 1c a9 ee 9b 16 d7 1d 83 6a

- No.: 5955
- Timestamp: 20:44:31:747_1
- RFN: 5615
- Chip: 30976
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 5956
- Timestamp: 20:44:31:748_0
- RFN: 5615
- Chip: 32000
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 5961
- Timestamp: 20:44:31:766_1
- RFN: 5617
- Chip: 27648
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 5985
- Timestamp: 20:44:31:818_0
- RFN: 5622
- Chip: 29952
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000110111'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'DBB6C71F29843F5322D0480BFECCE1'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 b9 1e db b6 c7 1f 29 84 3f 53 22 d0 48 0b fe cc e1

- No.: 5994
- Timestamp: 20:44:31:833_0
- RFN: 5624
- Chip: 9728
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 5995
- Timestamp: 20:44:31:833_1
- RFN: 5624
- Chip: 10752
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 5998
- Timestamp: 20:44:31:840_0
- RFN: 5625
- Chip: 512
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000110101'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = 'DEB6470A7EF3187C0CAB4475F232F8'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 ad 1e de b6 47 0a 7e f3 18 7c 0c ab 44 75 f2 32 f8

- No.: 6015
- Timestamp: 20:44:31:867_3
- RFN: 5627
- Chip: 28928
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 6018
- Timestamp: 20:44:31:871_1
- RFN: 5628
- Chip: 4608
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 6042
- Timestamp: 20:44:31:922_0
- RFN: 5633
- Chip: 7936
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000111000'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'E565DA36F8E6B0ED4E21AFC4CA1EFC'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 c1 1e e5 65 da 36 f8 e6 b0 ed 4e 21 af c4 ca 1e fc

- No.: 6051
- Timestamp: 20:44:31:936_0
- RFN: 5634
- Chip: 23040
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 6052
- Timestamp: 20:44:31:936_1
- RFN: 5634
- Chip: 23808
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 6055
- Timestamp: 20:44:31:943_0
- RFN: 5635
- Chip: 14336
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000110110'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '4C0B547758DC1CA9EE9B16D71D836A'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 b5 1e 4c 0b 54 77 58 dc 1c a9 ee 9b 16 d7 1d 83 6a

- No.: 6072
- Timestamp: 20:44:31:971_3
- RFN: 5638
- Chip: 7424
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 6075
- Timestamp: 20:44:31:976_1
- RFN: 5638
- Chip: 25856
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 6099
- Timestamp: 20:44:32:025_0
- RFN: 5643
- Chip: 22272
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000111001'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'E61A56F718D6B7127D0C81EA9BBC6C'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 c9 1e e6 1a 56 f7 18 d6 b7 12 7d 0c 81 ea 9b bc 6c

- No.: 6108
- Timestamp: 20:44:32:039_0
- RFN: 5644
- Chip: 37120
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 6109
- Timestamp: 20:44:32:039_1
- RFN: 5644
- Chip: 38144
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 6112
- Timestamp: 20:44:32:047_0
- RFN: 5645
- Chip: 28416
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000110111'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = 'DBB6C71F29843F5322D0480BFECCE1'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 bd 1e db b6 c7 1f 29 84 3f 53 22 d0 48 0b fe cc e1

- No.: 6129
- Timestamp: 20:44:32:076_0
- RFN: 5648
- Chip: 24832
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 6132
- Timestamp: 20:44:32:082_0
- RFN: 5649
- Chip: 11264
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000111000'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = 'E565DA36F8E6B0ED4E21AFC4CA1EFC'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 c5 1e e5 65 da 36 f8 e6 b0 ed 4e 21 af c4 ca 1e fc

- No.: 6149
- Timestamp: 20:44:32:109_0
- RFN: 5651
- Chip: 36352
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 6152
- Timestamp: 20:44:32:112_1
- RFN: 5652
- Chip: 12288
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 6176
- Timestamp: 20:44:32:161_0
- RFN: 5657
- Chip: 4096
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000111010'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'A4BA13A86EA4EF4E74F21856A2450A'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 d1 1e a4 ba 13 a8 6e a4 ef 4e 74 f2 18 56 a2 45 0a

- No.: 6185
- Timestamp: 20:44:32:177_1
- RFN: 5658
- Chip: 28160
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 6186
- Timestamp: 20:44:32:177_2
- RFN: 5658
- Chip: 29440
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 6189
- Timestamp: 20:44:32:185_0
- RFN: 5659
- Chip: 19968
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000111001'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = 'E61A56F718D6B7127D0C81EA9BBC6C'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 cd 1e e6 1a 56 f7 18 d6 b7 12 7d 0c 81 ea 9b bc 6c

- No.: 6206
- Timestamp: 20:44:32:212_2
- RFN: 5662
- Chip: 8960
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 6209
- Timestamp: 20:44:32:216_0
- RFN: 5662
- Chip: 23040
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 6233
- Timestamp: 20:44:32:263_0
- RFN: 5667
- Chip: 13824
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000111011'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '2BAEC4E0B012A8440A01002AAEEE4E'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 d9 1e 2b ae c4 e0 b0 12 a8 44 0a 01 00 2a ae ee 4e

- No.: 6242
- Timestamp: 20:44:32:277_1
- RFN: 5668
- Chip: 29696
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 6243
- Timestamp: 20:44:32:278_0
- RFN: 5668
- Chip: 31232
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 6248
- Timestamp: 20:44:32:302_1
- RFN: 5671
- Chip: 10240
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 6272
- Timestamp: 20:44:32:352_0
- RFN: 5676
- Chip: 10240
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000111100'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '5E5CF618FC19FC3352DD1C83407558'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 e1 1e 5e 5c f6 18 fc 19 fc 33 52 dd 1c 83 40 75 58

- No.: 6281
- Timestamp: 20:44:32:366_0
- RFN: 5677
- Chip: 25600
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 6282
- Timestamp: 20:44:32:366_1
- RFN: 5677
- Chip: 26624
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 6285
- Timestamp: 20:44:32:374_0
- RFN: 5678
- Chip: 17152
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000111010'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = 'A4BA13A86EA4EF4E74F21856A2450A'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 d5 1e a4 ba 13 a8 6e a4 ef 4e 74 f2 18 56 a2 45 0a

- No.: 6302
- Timestamp: 20:44:32:401_3
- RFN: 5681
- Chip: 7936
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 6305
- Timestamp: 20:44:32:406_0
- RFN: 5681
- Chip: 24832
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 6329
- Timestamp: 20:44:32:456_0
- RFN: 5686
- Chip: 23808
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000111101'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '8941757227AF3B2C7B5923D062A510'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 e9 1e 89 41 75 72 27 af 3b 2c 7b 59 23 d0 62 a5 10

- No.: 6338
- Timestamp: 20:44:32:470_1
- RFN: 5688
- Chip: 1536
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 6339
- Timestamp: 20:44:32:471_0
- RFN: 5688
- Chip: 2560
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 6342
- Timestamp: 20:44:32:478_0
- RFN: 5688
- Chip: 31488
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000111011'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '2BAEC4E0B012A8440A01002AAEEE4E'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 dd 1e 2b ae c4 e0 b0 12 a8 44 0a 01 00 2a ae ee 4e

- No.: 6359
- Timestamp: 20:44:32:506_1
- RFN: 5691
- Chip: 25344
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 6362
- Timestamp: 20:44:32:512_0
- RFN: 5692
- Chip: 6656
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 6386
- Timestamp: 20:44:32:560_0
- RFN: 5696
- Chip: 37888
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000111110'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '82BFB993C2CAE11A83BF933D2C84BF'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 f1 1e 82 bf b9 93 c2 ca e1 1a 83 bf 93 3d 2c 84 bf

- No.: 6395
- Timestamp: 20:44:32:573_1
- RFN: 5698
- Chip: 14592
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 6396
- Timestamp: 20:44:32:574_0
- RFN: 5698
- Chip: 15616
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 6399
- Timestamp: 20:44:32:581_0
- RFN: 5699
- Chip: 6144
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000111100'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '5E5CF618FC19FC3352DD1C83407558'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 e5 1e 5e 5c f6 18 fc 19 fc 33 52 dd 1c 83 40 75 58

- No.: 6416
- Timestamp: 20:44:32:611_3
- RFN: 5702
- Chip: 7168
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 6419
- Timestamp: 20:44:32:619_0
- RFN: 5702
- Chip: 36096
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000111101'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '8941757227AF3B2C7B5923D062A510'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 ed 1e 89 41 75 72 27 af 3b 2c 7b 59 23 d0 62 a5 10

- No.: 6436
- Timestamp: 20:44:32:646_1
- RFN: 5705
- Chip: 24320
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 6439
- Timestamp: 20:44:32:649_1
- RFN: 5705
- Chip: 38144
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 6463
- Timestamp: 20:44:32:697_0
- RFN: 5710
- Chip: 31744
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000111111'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '4675A76F24D0B7ED9B69242F51883E'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 f9 1e 46 75 a7 6f 24 d0 b7 ed 9b 69 24 2f 51 88 3e

- No.: 6472
- Timestamp: 20:44:32:714_1
- RFN: 5712
- Chip: 19712
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 6473
- Timestamp: 20:44:32:715_0
- RFN: 5712
- Chip: 20480
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 6476
- Timestamp: 20:44:32:722_0
- RFN: 5713
- Chip: 10496
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000111110'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '82BFB993C2CAE11A83BF933D2C84BF'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 f5 1e 82 bf b9 93 c2 ca e1 1a 83 bf 93 3d 2c 84 bf

- No.: 6493
- Timestamp: 20:44:32:749_3
- RFN: 5716
- Chip: 768
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 6496
- Timestamp: 20:44:32:754_1
- RFN: 5716
- Chip: 14848
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 6520
- Timestamp: 20:44:32:802_0
- RFN: 5721
- Chip: 7936
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001000000'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'ACEE1B03806AA445F5CDCB61257A26'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 01 1e ac ee 1b 03 80 6a a4 45 f5 cd cb 61 25 7a 26

- No.: 6529
- Timestamp: 20:44:32:816_0
- RFN: 5722
- Chip: 23296
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 6530
- Timestamp: 20:44:32:816_1
- RFN: 5722
- Chip: 24320
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 6535
- Timestamp: 20:44:32:842_1
- RFN: 5725
- Chip: 9216
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 6559
- Timestamp: 20:44:32:893_0
- RFN: 5730
- Chip: 12032
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001000001'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'FA4C5E09ABC460A545DF63252F7B26'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 09 1e fa 4c 5e 09 ab c4 60 a5 45 df 63 25 2f 7b 26

- No.: 6568
- Timestamp: 20:44:32:907_1
- RFN: 5731
- Chip: 29184
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 6569
- Timestamp: 20:44:32:908_0
- RFN: 5731
- Chip: 30720
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 6572
- Timestamp: 20:44:32:915_0
- RFN: 5732
- Chip: 20736
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000111111'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '4675A76F24D0B7ED9B69242F51883E'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 fd 1e 46 75 a7 6f 24 d0 b7 ed 9b 69 24 2f 51 88 3e

- No.: 6589
- Timestamp: 20:44:32:942_2
- RFN: 5735
- Chip: 10496
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 6592
- Timestamp: 20:44:32:946_1
- RFN: 5735
- Chip: 26624
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 6616
- Timestamp: 20:44:32:996_0
- RFN: 5740
- Chip: 27392
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001000010'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'D0E2B047F59896BDB9C69F167DA63A'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 11 1e d0 e2 b0 47 f5 98 96 bd b9 c6 9f 16 7d a6 3a

- No.: 6625
- Timestamp: 20:44:33:010_1
- RFN: 5742
- Chip: 4608
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 6626
- Timestamp: 20:44:33:011_0
- RFN: 5742
- Chip: 5632
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 6629
- Timestamp: 20:44:33:018_0
- RFN: 5742
- Chip: 35584
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001000000'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = 'ACEE1B03806AA445F5CDCB61257A26'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 05 1e ac ee 1b 03 80 6a a4 45 f5 cd cb 61 25 7a 26

- No.: 6646
- Timestamp: 20:44:33:049_1
- RFN: 5745
- Chip: 37120
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 6649
- Timestamp: 20:44:33:057_0
- RFN: 5746
- Chip: 28672
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001000001'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = 'FA4C5E09ABC460A545DF63252F7B26'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 0d 1e fa 4c 5e 09 ab c4 60 a5 45 df 63 25 2f 7b 26

- No.: 6666
- Timestamp: 20:44:33:085_0
- RFN: 5749
- Chip: 17920
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 6669
- Timestamp: 20:44:33:089_0
- RFN: 5749
- Chip: 33280
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 6693
- Timestamp: 20:44:33:136_0
- RFN: 5754
- Chip: 24832
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001000011'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '53A2C51F7CD9E3CF9E69A43A06FF19'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 19 1e 53 a2 c5 1f 7c d9 e3 cf 9e 69 a4 3a 06 ff 19

- No.: 6702
- Timestamp: 20:44:33:153_0
- RFN: 5756
- Chip: 12032
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 6703
- Timestamp: 20:44:33:153_1
- RFN: 5756
- Chip: 12800
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 6706
- Timestamp: 20:44:33:161_0
- RFN: 5757
- Chip: 3328
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001000010'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = 'D0E2B047F59896BDB9C69F167DA63A'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 15 1e d0 e2 b0 47 f5 98 96 bd b9 c6 9f 16 7d a6 3a

- No.: 6723
- Timestamp: 20:44:33:188_3
- RFN: 5759
- Chip: 32768
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 6726
- Timestamp: 20:44:33:192_0
- RFN: 5760
- Chip: 8192
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 6750
- Timestamp: 20:44:33:240_0
- RFN: 5765
- Chip: 512
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001000100'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '83C0600FFE665A5C5CA3452085408A'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 21 1e 83 c0 60 0f fe 66 5a 5c 5c a3 45 20 85 40 8a

- No.: 6759
- Timestamp: 20:44:33:254_0
- RFN: 5766
- Chip: 15616
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 6760
- Timestamp: 20:44:33:254_1
- RFN: 5766
- Chip: 16640
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 6765
- Timestamp: 20:44:33:277_1
- RFN: 5768
- Chip: 30208
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 6789
- Timestamp: 20:44:33:327_0
- RFN: 5773
- Chip: 30208
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001000101'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'BEECE4B0B813FD337873F2CD1E29AE'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 29 1e be ec e4 b0 b8 13 fd 33 78 73 f2 cd 1e 29 ae

- No.: 6798
- Timestamp: 20:44:33:341_1
- RFN: 5775
- Chip: 7936
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 6799
- Timestamp: 20:44:33:341_2
- RFN: 5775
- Chip: 8704
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 6802
- Timestamp: 20:44:33:349_0
- RFN: 5775
- Chip: 37888
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001000011'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '53A2C51F7CD9E3CF9E69A43A06FF19'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 1d 1e 53 a2 c5 1f 7c d9 e3 cf 9e 69 a4 3a 06 ff 19

- No.: 6819
- Timestamp: 20:44:33:376_4
- RFN: 5778
- Chip: 28416
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 6822
- Timestamp: 20:44:33:381_1
- RFN: 5779
- Chip: 4096
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 6846
- Timestamp: 20:44:33:431_0
- RFN: 5784
- Chip: 4096
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001000110'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '91BD6C8E14FDE630F8195688EBE465'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 31 1e 91 bd 6c 8e 14 fd e6 30 f8 19 56 88 eb e4 65

- No.: 6855
- Timestamp: 20:44:33:445_1
- RFN: 5785
- Chip: 19968
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 6856
- Timestamp: 20:44:33:445_2
- RFN: 5785
- Chip: 20992
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 6859
- Timestamp: 20:44:33:453_0
- RFN: 5786
- Chip: 12288
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001000100'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '83C0600FFE665A5C5CA3452085408A'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 25 1e 83 c0 60 0f fe 66 5a 5c 5c a3 45 20 85 40 8a

- No.: 6876
- Timestamp: 20:44:33:483_2
- RFN: 5789
- Chip: 12800
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 6879
- Timestamp: 20:44:33:491_0
- RFN: 5790
- Chip: 3584
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001000101'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = 'BEECE4B0B813FD337873F2CD1E29AE'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 2d 1e be ec e4 b0 b8 13 fd 33 78 73 f2 cd 1e 29 ae

- No.: 6896
- Timestamp: 20:44:33:517_3
- RFN: 5792
- Chip: 29696
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 6899
- Timestamp: 20:44:33:521_1
- RFN: 5793
- Chip: 6144
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 6923
- Timestamp: 20:44:33:569_0
- RFN: 5797
- Chip: 35328
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001000111'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'F09816A8EEB1B83953DD362DAE3B06'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 39 1e f0 98 16 a8 ee b1 b8 39 53 dd 36 2d ae 3b 06

- No.: 6932
- Timestamp: 20:44:33:583_0
- RFN: 5799
- Chip: 12800
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 6933
- Timestamp: 20:44:33:583_1
- RFN: 5799
- Chip: 13568
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 6938
- Timestamp: 20:44:33:597_0
- RFN: 5800
- Chip: 31232
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001000110'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '91BD6C8E14FDE630F8195688EBE465'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 35 1e 91 bd 6c 8e 14 fd e6 30 f8 19 56 88 eb e4 65

- No.: 6955
- Timestamp: 20:44:33:625_0
- RFN: 5803
- Chip: 20736
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 6958
- Timestamp: 20:44:33:628_1
- RFN: 5803
- Chip: 34560
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 6982
- Timestamp: 20:44:33:676_0
- RFN: 5808
- Chip: 26624
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001001000'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'D5B76D8E3E53087EA645A09017FD99'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 41 1e d5 b7 6d 8e 3e 53 08 7e a6 45 a0 90 17 fd 99

- No.: 6991
- Timestamp: 20:44:33:690_1
- RFN: 5810
- Chip: 3840
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 6992
- Timestamp: 20:44:33:690_2
- RFN: 5810
- Chip: 4864
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 6997
- Timestamp: 20:44:33:705_1
- RFN: 5811
- Chip: 19456
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 7021
- Timestamp: 20:44:33:755_0
- RFN: 5816
- Chip: 21504
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001001001'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'C3CACBB46DF1CD61DA9C435F89943D'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 49 1e c3 ca cb b4 6d f1 cd 61 da 9c 43 5f 89 94 3d

- No.: 7030
- Timestamp: 20:44:33:769_1
- RFN: 5817
- Chip: 36864
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 7031
- Timestamp: 20:44:33:770_0
- RFN: 5817
- Chip: 37632
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 7034
- Timestamp: 20:44:33:777_0
- RFN: 5818
- Chip: 28672
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001000111'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = 'F09816A8EEB1B83953DD362DAE3B06'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 3d 1e f0 98 16 a8 ee b1 b8 39 53 dd 36 2d ae 3b 06

- No.: 7051
- Timestamp: 20:44:33:815_0
- RFN: 5822
- Chip: 18944
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 7054
- Timestamp: 20:44:33:818_1
- RFN: 5822
- Chip: 32256
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 7078
- Timestamp: 20:44:33:871_0
- RFN: 5828
- Chip: 4352
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001001010'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'F9CC34ADEE31AD6E24FA1903D53778'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 51 1e f9 cc 34 ad ee 31 ad 6e 24 fa 19 03 d5 37 78

- No.: 7087
- Timestamp: 20:44:33:884_1
- RFN: 5829
- Chip: 20992
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 7088
- Timestamp: 20:44:33:885_0
- RFN: 5829
- Chip: 22016
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 7091
- Timestamp: 20:44:33:893_0
- RFN: 5830
- Chip: 12544
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001001000'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = 'D5B76D8E3E53087EA645A09017FD99'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 45 1e d5 b7 6d 8e 3e 53 08 7e a6 45 a0 90 17 fd 99

- No.: 7108
- Timestamp: 20:44:33:923_0
- RFN: 5833
- Chip: 12544
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 7111
- Timestamp: 20:44:33:930_0
- RFN: 5834
- Chip: 2560
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001001001'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = 'C3CACBB46DF1CD61DA9C435F89943D'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 4d 1e c3 ca cb b4 6d f1 cd 61 da 9c 43 5f 89 94 3d

- No.: 7128
- Timestamp: 20:44:33:957_2
- RFN: 5836
- Chip: 30720
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 7131
- Timestamp: 20:44:33:961_0
- RFN: 5837
- Chip: 5888
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 7155
- Timestamp: 20:44:34:009_0
- RFN: 5841
- Chip: 36352
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001001011'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'D949742750DD49DE9CE9E430AD448A'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 59 1e d9 49 74 27 50 dd 49 de 9c e9 e4 30 ad 44 8a

- No.: 7164
- Timestamp: 20:44:34:024_0
- RFN: 5843
- Chip: 15616
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 7165
- Timestamp: 20:44:34:024_1
- RFN: 5843
- Chip: 16384
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 7170
- Timestamp: 20:44:34:038_0
- RFN: 5844
- Chip: 29952
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001001010'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = 'F9CC34ADEE31AD6E24FA1903D53778'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 55 1e f9 cc 34 ad ee 31 ad 6e 24 fa 19 03 d5 37 78

- No.: 7187
- Timestamp: 20:44:34:065_3
- RFN: 5847
- Chip: 20736
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 7190
- Timestamp: 20:44:34:069_1
- RFN: 5847
- Chip: 34560
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 7214
- Timestamp: 20:44:34:116_0
- RFN: 5852
- Chip: 26112
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001001100'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '14575D89C160255088140200555DDC'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 61 1e 14 57 5d 89 c1 60 25 50 88 14 02 00 55 5d dc

- No.: 7223
- Timestamp: 20:44:34:130_1
- RFN: 5854
- Chip: 2048
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 7224
- Timestamp: 20:44:34:131_0
- RFN: 5854
- Chip: 3328
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 7229
- Timestamp: 20:44:34:146_1
- RFN: 5855
- Chip: 26368
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 7253
- Timestamp: 20:44:34:196_0
- RFN: 5860
- Chip: 26112
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001001101'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '9CBCB9EC31F833F866A5BA390680EA'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 69 1e 9c bc b9 ec 31 f8 33 f8 66 a5 ba 39 06 80 ea

- No.: 7262
- Timestamp: 20:44:34:210_1
- RFN: 5862
- Chip: 3328
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 7263
- Timestamp: 20:44:34:211_0
- RFN: 5862
- Chip: 4352
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 7266
- Timestamp: 20:44:34:218_0
- RFN: 5862
- Chip: 33024
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001001011'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = 'D949742750DD49DE9CE9E430AD448A'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 5d 1e d9 49 74 27 50 dd 49 de 9c e9 e4 30 ad 44 8a

- No.: 7283
- Timestamp: 20:44:34:245_3
- RFN: 5865
- Chip: 22784
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 7286
- Timestamp: 20:44:34:249_1
- RFN: 5865
- Chip: 37120
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 7310
- Timestamp: 20:44:34:299_0
- RFN: 5871
- Chip: 1280
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001001110'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'B11282EAE44F5E7658F6B247A0C54A'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 71 1e b1 12 82 ea e4 4f 5e 76 58 f6 b2 47 a0 c5 4a

- No.: 7319
- Timestamp: 20:44:34:314_0
- RFN: 5872
- Chip: 18176
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 7320
- Timestamp: 20:44:34:314_1
- RFN: 5872
- Chip: 19200
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 7323
- Timestamp: 20:44:34:322_0
- RFN: 5873
- Chip: 8448
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001001100'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '14575D89C160255088140200555DDC'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 65 1e 14 57 5d 89 c1 60 25 50 88 14 02 00 55 5d dc

- No.: 7340
- Timestamp: 20:44:34:352_3
- RFN: 5876
- Chip: 8960
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 7343
- Timestamp: 20:44:34:360_0
- RFN: 5876
- Chip: 37376
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001001101'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '9CBCB9EC31F833F866A5BA390680EA'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 6d 1e 9c bc b9 ec 31 f8 33 f8 66 a5 ba 39 06 80 ea

- No.: 7360
- Timestamp: 20:44:34:387_2
- RFN: 5879
- Chip: 27648
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 7363
- Timestamp: 20:44:34:391_0
- RFN: 5880
- Chip: 3584
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 7387
- Timestamp: 20:44:34:438_0
- RFN: 5884
- Chip: 33536
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001001111'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '21057F73278595C235077F267A5909'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 79 1e 21 05 7f 73 27 85 95 c2 35 07 7f 26 7a 59 09

- No.: 7396
- Timestamp: 20:44:34:455_0
- RFN: 5886
- Chip: 19200
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 7397
- Timestamp: 20:44:34:455_1
- RFN: 5886
- Chip: 19968
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 7400
- Timestamp: 20:44:34:463_0
- RFN: 5887
- Chip: 13568
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001001110'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = 'B11282EAE44F5E7658F6B247A0C54A'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 75 1e b1 12 82 ea e4 4f 5e 76 58 f6 b2 47 a0 c5 4a

- No.: 7417
- Timestamp: 20:44:34:490_3
- RFN: 5890
- Chip: 3072
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 7420
- Timestamp: 20:44:34:494_1
- RFN: 5890
- Chip: 17664
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 7444
- Timestamp: 20:44:34:542_0
- RFN: 5895
- Chip: 9728
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001010000'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '7E8CEB4EDE49A16FDB36D2485EA310'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 81 1e 7e 8c eb 4e de 49 a1 6f db 36 d2 48 5e a3 10

- No.: 7453
- Timestamp: 20:44:34:556_0
- RFN: 5896
- Chip: 25600
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 7454
- Timestamp: 20:44:34:556_1
- RFN: 5896
- Chip: 26368
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 7459
- Timestamp: 20:44:34:573_1
- RFN: 5898
- Chip: 13824
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 7483
- Timestamp: 20:44:34:622_0
- RFN: 5903
- Chip: 12544
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001010001'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '7D59DC360700D5488BEB9B96C24AF4'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 89 1e 7d 59 dc 36 07 00 d5 48 8b eb 9b 96 c2 4a f4

- No.: 7492
- Timestamp: 20:44:34:637_1
- RFN: 5904
- Chip: 27904
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 7493
- Timestamp: 20:44:34:638_0
- RFN: 5904
- Chip: 28672
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 7496
- Timestamp: 20:44:34:645_0
- RFN: 5905
- Chip: 19456
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001001111'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '21057F73278595C235077F267A5909'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 7d 1e 21 05 7f 73 27 85 95 c2 35 07 7f 26 7a 59 09

- No.: 7513
- Timestamp: 20:44:34:672_4
- RFN: 5908
- Chip: 9728
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 7516
- Timestamp: 20:44:34:676_1
- RFN: 5908
- Chip: 24320
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 7540
- Timestamp: 20:44:34:726_0
- RFN: 5913
- Chip: 25088
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001010010'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '4DF498BC135788C14A8BBEC64A5EF6'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 91 1e 4d f4 98 bc 13 57 88 c1 4a 8b be c6 4a 5e f6

- No.: 7549
- Timestamp: 20:44:34:740_1
- RFN: 5915
- Chip: 3072
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 7550
- Timestamp: 20:44:34:741_0
- RFN: 5915
- Chip: 4096
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 7553
- Timestamp: 20:44:34:748_0
- RFN: 5915
- Chip: 33024
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001010000'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '7E8CEB4EDE49A16FDB36D2485EA310'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 85 1e 7e 8c eb 4e de 49 a1 6f db 36 d2 48 5e a3 10

- No.: 7570
- Timestamp: 20:44:34:778_3
- RFN: 5918
- Chip: 33280
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 7573
- Timestamp: 20:44:34:787_0
- RFN: 5919
- Chip: 29440
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001010001'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '7D59DC360700D5488BEB9B96C24AF4'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 8d 1e 7d 59 dc 36 07 00 d5 48 8b eb 9b 96 c2 4a f4

- No.: 7590
- Timestamp: 20:44:34:814_1
- RFN: 5922
- Chip: 16384
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 7593
- Timestamp: 20:44:34:817_1
- RFN: 5922
- Chip: 30720
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 7617
- Timestamp: 20:44:34:866_0
- RFN: 5927
- Chip: 24064
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001010011'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '4DA1C5608FEB312D7B738D3E2CFB4C'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 99 1e 4d a1 c5 60 8f eb 31 2d 7b 73 8d 3e 2c fb 4c

- No.: 7626
- Timestamp: 20:44:34:879_1
- RFN: 5929
- Chip: 0
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 7627
- Timestamp: 20:44:34:880_0
- RFN: 5929
- Chip: 1280
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 7632
- Timestamp: 20:44:34:895_0
- RFN: 5930
- Chip: 22528
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001010010'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '4DF498BC135788C14A8BBEC64A5EF6'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 95 1e 4d f4 98 bc 13 57 88 c1 4a 8b be c6 4a 5e f6

- No.: 7649
- Timestamp: 20:44:34:922_3
- RFN: 5933
- Chip: 12288
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 7652
- Timestamp: 20:44:34:926_1
- RFN: 5933
- Chip: 27136
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 7676
- Timestamp: 20:44:34:975_0
- RFN: 5938
- Chip: 19200
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001010100'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '74A7458A3EF9B3C79F3CD348740DFE'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 a1 1e 74 a7 45 8a 3e f9 b3 c7 9f 3c d3 48 74 0d fe

- No.: 7685
- Timestamp: 20:44:34:989_0
- RFN: 5939
- Chip: 34048
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 7686
- Timestamp: 20:44:34:989_1
- RFN: 5939
- Chip: 35072
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 7691
- Timestamp: 20:44:35:015_0
- RFN: 5942
- Chip: 20480
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001010011'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '4DA1C5608FEB312D7B738D3E2CFB4C'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 9d 1e 4d a1 c5 60 8f eb 31 2d 7b 73 8d 3e 2c fb 4c

- No.: 7708
- Timestamp: 20:44:35:043_0
- RFN: 5945
- Chip: 11008
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 7711
- Timestamp: 20:44:35:046_1
- RFN: 5945
- Chip: 24832
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 7735
- Timestamp: 20:44:35:094_0
- RFN: 5950
- Chip: 18176
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001010101'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '330780C01FFCCCB4B8B9468A410A81'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 a9 1e 33 07 80 c0 1f fc cc b4 b8 b9 46 8a 41 0a 81

- No.: 7744
- Timestamp: 20:44:35:108_1
- RFN: 5951
- Chip: 33792
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 7745
- Timestamp: 20:44:35:109_0
- RFN: 5951
- Chip: 34560
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 7750
- Timestamp: 20:44:35:135_0
- RFN: 5954
- Chip: 20736
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001010100'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '74A7458A3EF9B3C79F3CD348740DFE'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 a5 1e 74 a7 45 8a 3e f9 b3 c7 9f 3c d3 48 74 0d fe

- No.: 7767
- Timestamp: 20:44:35:162_0
- RFN: 5957
- Chip: 8448
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 7770
- Timestamp: 20:44:35:165_1
- RFN: 5957
- Chip: 23040
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 7794
- Timestamp: 20:44:35:213_0
- RFN: 5962
- Chip: 15872
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001010110'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '157DD9C9617027FA66F0E7E59A3C53'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 b1 1e 15 7d d9 c9 61 70 27 fa 66 f0 e7 e5 9a 3c 53

- No.: 7803
- Timestamp: 20:44:35:227_1
- RFN: 5963
- Chip: 32000
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 7804
- Timestamp: 20:44:35:228_0
- RFN: 5963
- Chip: 33024
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 7809
- Timestamp: 20:44:35:250_1
- RFN: 5966
- Chip: 3584
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 7833
- Timestamp: 20:44:35:300_0
- RFN: 5970
- Chip: 37120
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001010111'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '5D237AD91C29FBCC61F032AD11D7C8'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 b9 1e 5d 23 7a d9 1c 29 fb cc 61 f0 32 ad 11 d7 c8

- No.: 7842
- Timestamp: 20:44:35:313_1
- RFN: 5972
- Chip: 13824
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 7843
- Timestamp: 20:44:35:314_0
- RFN: 5972
- Chip: 14848
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 7846
- Timestamp: 20:44:35:321_0
- RFN: 5973
- Chip: 5376
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001010101'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '330780C01FFCCCB4B8B9468A410A81'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 ad 1e 33 07 80 c0 1f fc cc b4 b8 b9 46 8a 41 0a 81

- No.: 7863
- Timestamp: 20:44:35:349_1
- RFN: 5975
- Chip: 34816
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 7866
- Timestamp: 20:44:35:352_1
- RFN: 5976
- Chip: 9728
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 7890
- Timestamp: 20:44:35:402_0
- RFN: 5981
- Chip: 10240
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001011000'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'CBE1302D51DD637072A7BA6C5B5C76'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 c1 1e cb e1 30 2d 51 dd 63 70 72 a7 ba 6c 5b 5c 76

- No.: 7899
- Timestamp: 20:44:35:417_0
- RFN: 5982
- Chip: 26880
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 7900
- Timestamp: 20:44:35:417_1
- RFN: 5982
- Chip: 28160
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 7903
- Timestamp: 20:44:35:424_0
- RFN: 5983
- Chip: 18432
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001010110'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '157DD9C9617027FA66F0E7E59A3C53'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 b5 1e 15 7d d9 c9 61 70 27 fa 66 f0 e7 e5 9a 3c 53

- No.: 7920
- Timestamp: 20:44:35:454_2
- RFN: 5986
- Chip: 18432
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 7923
- Timestamp: 20:44:35:462_0
- RFN: 5987
- Chip: 9472
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001010111'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '5D237AD91C29FBCC61F032AD11D7C8'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 bd 1e 5d 23 7a d9 1c 29 fb cc 61 f0 32 ad 11 d7 c8

- No.: 7940
- Timestamp: 20:44:35:489_2
- RFN: 5989
- Chip: 37888
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 7943
- Timestamp: 20:44:35:493_0
- RFN: 5990
- Chip: 13056
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 7967
- Timestamp: 20:44:35:541_0
- RFN: 5995
- Chip: 5888
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001011001'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '0DAB6EDB1C7CA610FD4C8B41202FFB'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 c9 1e 0d ab 6e db 1c 7c a6 10 fd 4c 8b 41 20 2f fb

- No.: 7976
- Timestamp: 20:44:35:557_1
- RFN: 5996
- Chip: 30976
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 7977
- Timestamp: 20:44:35:557_2
- RFN: 5996
- Chip: 31744
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 7980
- Timestamp: 20:44:35:565_0
- RFN: 5997
- Chip: 23040
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001011000'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = 'CBE1302D51DD637072A7BA6C5B5C76'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 c5 1e cb e1 30 2d 51 dd 63 70 72 a7 ba 6c 5b 5c 76

- No.: 7997
- Timestamp: 20:44:35:593_3
- RFN: 6000
- Chip: 12544
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 8000
- Timestamp: 20:44:35:597_1
- RFN: 6000
- Chip: 27392
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 8024
- Timestamp: 20:44:35:644_0
- RFN: 6005
- Chip: 17152
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001011010'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '3387959768DBE39AC3B53886BF1328'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 d1 1e 33 87 95 97 68 db e3 9a c3 b5 38 86 bf 13 28

- No.: 8033
- Timestamp: 20:44:35:658_1
- RFN: 6006
- Chip: 32256
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 8034
- Timestamp: 20:44:35:658_2
- RFN: 6006
- Chip: 33280
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 8039
- Timestamp: 20:44:35:683_1
- RFN: 6009
- Chip: 12800
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 8063
- Timestamp: 20:44:35:733_0
- RFN: 6014
- Chip: 12032
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001011011'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '7BF398695BDC635ADC49F43207AA6E'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 d9 1e 7b f3 98 69 5b dc 63 5a dc 49 f4 32 07 aa 6e

- No.: 8072
- Timestamp: 20:44:35:747_0
- RFN: 6015
- Chip: 29184
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 8073
- Timestamp: 20:44:35:747_1
- RFN: 6015
- Chip: 30208
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 8076
- Timestamp: 20:44:35:755_0
- RFN: 6016
- Chip: 20224
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001011001'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '0DAB6EDB1C7CA610FD4C8B41202FFB'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 cd 1e 0d ab 6e db 1c 7c a6 10 fd 4c 8b 41 20 2f fb

- No.: 8093
- Timestamp: 20:44:35:782_1
- RFN: 6019
- Chip: 9728
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 8096
- Timestamp: 20:44:35:789_1
- RFN: 6019
- Chip: 37120
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 8120
- Timestamp: 20:44:35:837_0
- RFN: 6024
- Chip: 30208
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001011100'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'F1B292E84EA1BA93BD39D3C8615A89'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 e1 1e f1 b2 92 e8 4e a1 ba 93 bd 39 d3 c8 61 5a 89

- No.: 8129
- Timestamp: 20:44:35:851_0
- RFN: 6026
- Chip: 6912
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 8130
- Timestamp: 20:44:35:851_1
- RFN: 6026
- Chip: 7936
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 8133
- Timestamp: 20:44:35:859_0
- RFN: 6026
- Chip: 37376
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001011010'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '3387959768DBE39AC3B53886BF1328'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 d5 1e 33 87 95 97 68 db e3 9a c3 b5 38 86 bf 13 28

- No.: 8150
- Timestamp: 20:44:35:890_0
- RFN: 6029
- Chip: 37120
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 8153
- Timestamp: 20:44:35:897_0
- RFN: 6030
- Chip: 27904
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001011011'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '7BF398695BDC635ADC49F43207AA6E'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 dd 1e 7b f3 98 69 5b dc 63 5a dc 49 f4 32 07 aa 6e

- No.: 8170
- Timestamp: 20:44:35:926_1
- RFN: 6033
- Chip: 22272
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 8173
- Timestamp: 20:44:35:929_1
- RFN: 6033
- Chip: 35328
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 8197
- Timestamp: 20:44:35:977_0
- RFN: 6038
- Chip: 27136
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001011101'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '1428AEBB1382C04AA110280400AABB'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 e9 1e 14 28 ae bb 13 82 c0 4a a1 10 28 04 00 aa bb

- No.: 8206
- Timestamp: 20:44:35:993_1
- RFN: 6040
- Chip: 13312
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 8207
- Timestamp: 20:44:35:993_2
- RFN: 6040
- Chip: 14336
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 8210
- Timestamp: 20:44:36:001_0
- RFN: 6041
- Chip: 4608
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001011100'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = 'F1B292E84EA1BA93BD39D3C8615A89'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 e5 1e f1 b2 92 e8 4e a1 ba 93 bd 39 d3 c8 61 5a 89

- No.: 8227
- Timestamp: 20:44:36:029_1
- RFN: 6043
- Chip: 35328
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 8230
- Timestamp: 20:44:36:032_1
- RFN: 6044
- Chip: 11520
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 8254
- Timestamp: 20:44:36:080_0
- RFN: 6049
- Chip: 1792
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001011110'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'B9397973D863F067F0CD4B74720D01'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 f1 1e b9 39 79 73 d8 63 f0 67 f0 cd 4b 74 72 0d 01

- No.: 8263
- Timestamp: 20:44:36:094_0
- RFN: 6050
- Chip: 16896
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 8264
- Timestamp: 20:44:36:094_1
- RFN: 6050
- Chip: 17664
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 8269
- Timestamp: 20:44:36:117_1
- RFN: 6052
- Chip: 30208
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 8293
- Timestamp: 20:44:36:167_0
- RFN: 6057
- Chip: 30464
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001011111'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'D5622505D5C89EBCECB1ED648F418A'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 f9 1e d5 62 25 05 d5 c8 9e bc ec b1 ed 64 8f 41 8a

- No.: 8302
- Timestamp: 20:44:36:181_1
- RFN: 6059
- Chip: 8192
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 8303
- Timestamp: 20:44:36:182_0
- RFN: 6059
- Chip: 9472
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 8306
- Timestamp: 20:44:36:189_0
- RFN: 6060
- Chip: 256
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001011101'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '1428AEBB1382C04AA110280400AABB'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 ed 1e 14 28 ae bb 13 82 c0 4a a1 10 28 04 00 aa bb

- No.: 8323
- Timestamp: 20:44:36:217_3
- RFN: 6062
- Chip: 28416
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 8326
- Timestamp: 20:44:36:221_1
- RFN: 6063
- Chip: 4608
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 8350
- Timestamp: 20:44:36:272_0
- RFN: 6068
- Chip: 8448
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001100000'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '94420AFEE64F0B2B846A0EFE4CF4B2'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 01 1e 94 42 0a fe e6 4f 0b 2b 84 6a 0e fe 4c f4 b2

- No.: 8359
- Timestamp: 20:44:36:286_1
- RFN: 6069
- Chip: 24320
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 8360
- Timestamp: 20:44:36:286_2
- RFN: 6069
- Chip: 25344
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 8363
- Timestamp: 20:44:36:294_0
- RFN: 6070
- Chip: 16128
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001011110'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = 'B9397973D863F067F0CD4B74720D01'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 f5 1e b9 39 79 73 d8 63 f0 67 f0 cd 4b 74 72 0d 01

- No.: 8380
- Timestamp: 20:44:36:324_0
- RFN: 6073
- Chip: 15360
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 8383
- Timestamp: 20:44:36:331_0
- RFN: 6074
- Chip: 5888
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001011111'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = 'D5622505D5C89EBCECB1ED648F418A'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 82 fd 1e d5 62 25 05 d5 c8 9e bc ec b1 ed 64 8f 41 8a

- No.: 8400
- Timestamp: 20:44:36:358_2
- RFN: 6076
- Chip: 33280
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 8403
- Timestamp: 20:44:36:362_0
- RFN: 6077
- Chip: 9216
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 8427
- Timestamp: 20:44:36:410_0
- RFN: 6082
- Chip: 2304
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001100001'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '12FD19D69DBC9342DFB66DA490BD46'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 09 1e 12 fd 19 d6 9d bc 93 42 df b6 6d a4 90 bd 46

- No.: 8436
- Timestamp: 20:44:36:424_1
- RFN: 6083
- Chip: 19712
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 8437
- Timestamp: 20:44:36:425_0
- RFN: 6083
- Chip: 20736
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 8440
- Timestamp: 20:44:36:435_0
- RFN: 6084
- Chip: 20992
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001100000'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '94420AFEE64F0B2B846A0EFE4CF4B2'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 05 1e 94 42 0a fe e6 4f 0b 2b 84 6a 0e fe 4c f4 b2

- No.: 8457
- Timestamp: 20:44:36:462_3
- RFN: 6087
- Chip: 12032
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 8460
- Timestamp: 20:44:36:466_1
- RFN: 6087
- Chip: 27392
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 8484
- Timestamp: 20:44:36:515_0
- RFN: 6092
- Chip: 18944
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001100010'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '20FAB3B86C0E01AA9117D7372D8495'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 11 1e 20 fa b3 b8 6c 0e 01 aa 91 17 d7 37 2d 84 95

- No.: 8493
- Timestamp: 20:44:36:529_0
- RFN: 6093
- Chip: 34048
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 8494
- Timestamp: 20:44:36:529_1
- RFN: 6093
- Chip: 35072
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 8499
- Timestamp: 20:44:36:547_1
- RFN: 6095
- Chip: 27136
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 8523
- Timestamp: 20:44:36:597_0
- RFN: 6100
- Chip: 28416
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001100011'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'E89BE9317826AF118295177D8C94BD'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 19 1e e8 9b e9 31 78 26 af 11 82 95 17 7d 8c 94 bd

- No.: 8532
- Timestamp: 20:44:36:612_0
- RFN: 6102
- Chip: 8192
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 8533
- Timestamp: 20:44:36:612_1
- RFN: 6102
- Chip: 9216
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 8536
- Timestamp: 20:44:36:619_0
- RFN: 6102
- Chip: 37632
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001100001'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '12FD19D69DBC9342DFB66DA490BD46'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 0d 1e 12 fd 19 d6 9d bc 93 42 df b6 6d a4 90 bd 46

- No.: 8553
- Timestamp: 20:44:36:647_0
- RFN: 6105
- Chip: 27392
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 8556
- Timestamp: 20:44:36:650_1
- RFN: 6106
- Chip: 3072
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 8580
- Timestamp: 20:44:36:701_0
- RFN: 6111
- Chip: 5888
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001100100'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'EC9B438AC11FD6625AF6E71A7C59F6'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 21 1e ec 9b 43 8a c1 1f d6 62 5a f6 e7 1a 7c 59 f6

- No.: 8589
- Timestamp: 20:44:36:715_0
- RFN: 6112
- Chip: 20992
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 8590
- Timestamp: 20:44:36:715_1
- RFN: 6112
- Chip: 22016
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 8593
- Timestamp: 20:44:36:723_0
- RFN: 6113
- Chip: 13824
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001100010'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '20FAB3B86C0E01AA9117D7372D8495'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 15 1e 20 fa b3 b8 6c 0e 01 aa 91 17 d7 37 2d 84 95

- No.: 8610
- Timestamp: 20:44:36:752_2
- RFN: 6116
- Chip: 10240
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 8613
- Timestamp: 20:44:36:760_0
- RFN: 6117
- Chip: 2048
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001100011'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = 'E89BE9317826AF118295177D8C94BD'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 1d 1e e8 9b e9 31 78 26 af 11 82 95 17 7d 8c 94 bd

- No.: 8630
- Timestamp: 20:44:36:788_2
- RFN: 6119
- Chip: 34304
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 8633
- Timestamp: 20:44:36:792_1
- RFN: 6120
- Chip: 11264
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 8657
- Timestamp: 20:44:36:841_0
- RFN: 6125
- Chip: 2560
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001100101'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '98E94E8B147DF3678F3E79A690E81B'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 29 1e 98 e9 4e 8b 14 7d f3 67 8f 3e 79 a6 90 e8 1b

- No.: 8666
- Timestamp: 20:44:36:857_1
- RFN: 6126
- Chip: 27392
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 8667
- Timestamp: 20:44:36:857_2
- RFN: 6126
- Chip: 28160
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 8670
- Timestamp: 20:44:36:865_0
- RFN: 6127
- Chip: 18688
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001100100'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = 'EC9B438AC11FD6625AF6E71A7C59F6'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 25 1e ec 9b 43 8a c1 1f d6 62 5a f6 e7 1a 7c 59 f6

- No.: 8687
- Timestamp: 20:44:36:893_0
- RFN: 6130
- Chip: 10240
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 8690
- Timestamp: 20:44:36:896_1
- RFN: 6130
- Chip: 24320
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 8714
- Timestamp: 20:44:36:945_0
- RFN: 6135
- Chip: 20224
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001100110'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'FC660F01803FF9996971728D148215'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 31 1e fc 66 0f 01 80 3f f9 99 69 71 72 8d 14 82 15

- No.: 8723
- Timestamp: 20:44:36:959_0
- RFN: 6136
- Chip: 35072
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 8724
- Timestamp: 20:44:36:959_1
- RFN: 6136
- Chip: 35840
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 8729
- Timestamp: 20:44:36:976_1
- RFN: 6138
- Chip: 25088
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 8753
- Timestamp: 20:44:37:026_0
- RFN: 6143
- Chip: 26368
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001100111'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '022AFBB392C2E04FF4CDE1CFCB3478'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 39 1e 02 2a fb b3 92 c2 e0 4f f4 cd e1 cf cb 34 78

- No.: 8762
- Timestamp: 20:44:37:041_0
- RFN: 6145
- Chip: 4864
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 8763
- Timestamp: 20:44:37:041_1
- RFN: 6145
- Chip: 6144
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 8766
- Timestamp: 20:44:37:048_0
- RFN: 6145
- Chip: 34816
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001100101'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '98E94E8B147DF3678F3E79A690E81B'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 2d 1e 98 e9 4e 8b 14 7d f3 67 8f 3e 79 a6 90 e8 1b

- No.: 8783
- Timestamp: 20:44:37:076_2
- RFN: 6148
- Chip: 26368
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 8786
- Timestamp: 20:44:37:080_0
- RFN: 6149
- Chip: 1792
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 8810
- Timestamp: 20:44:37:130_0
- RFN: 6154
- Chip: 2816
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001101000'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'A6BA46F5B23853F798C3E0655A23AF'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 41 1e a6 ba 46 f5 b2 38 53 f7 98 c3 e0 65 5a 23 af

- No.: 8819
- Timestamp: 20:44:37:145_0
- RFN: 6155
- Chip: 18432
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 8820
- Timestamp: 20:44:37:145_1
- RFN: 6155
- Chip: 19456
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 8823
- Timestamp: 20:44:37:152_0
- RFN: 6156
- Chip: 9472
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001100110'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = 'FC660F01803FF9996971728D148215'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 35 1e fc 66 0f 01 80 3f f9 99 69 71 72 8d 14 82 15

- No.: 8840
- Timestamp: 20:44:37:182_4
- RFN: 6159
- Chip: 9728
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 8843
- Timestamp: 20:44:37:190_0
- RFN: 6160
- Chip: 256
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001100111'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '022AFBB392C2E04FF4CDE1CFCB3478'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 3d 1e 02 2a fb b3 92 c2 e0 4f f4 cd e1 cf cb 34 78

- No.: 8860
- Timestamp: 20:44:37:217_1
- RFN: 6162
- Chip: 27136
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 8863
- Timestamp: 20:44:37:221_0
- RFN: 6163
- Chip: 3840
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 8887
- Timestamp: 20:44:37:269_0
- RFN: 6167
- Chip: 35584
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001101001'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '9197C2605AA3BAC6E0E54F74D8B6B8'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 49 1e 91 97 c2 60 5a a3 ba c6 e0 e5 4f 74 d8 b6 b8

- No.: 8896
- Timestamp: 20:44:37:283_1
- RFN: 6169
- Chip: 14592
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 8897
- Timestamp: 20:44:37:284_0
- RFN: 6169
- Chip: 15616
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 8902
- Timestamp: 20:44:37:297_0
- RFN: 6170
- Chip: 29440
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001101000'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = 'A6BA46F5B23853F798C3E0655A23AF'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 45 1e a6 ba 46 f5 b2 38 53 f7 98 c3 e0 65 5a 23 af

- No.: 8919
- Timestamp: 20:44:37:325_0
- RFN: 6173
- Chip: 19968
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 8922
- Timestamp: 20:44:37:328_1
- RFN: 6173
- Chip: 34048
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 8946
- Timestamp: 20:44:37:376_0
- RFN: 6178
- Chip: 25600
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001101010'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'EC1B56DDB638F94C21FA991682405F'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 51 1e ec 1b 56 dd b6 38 f9 4c 21 fa 99 16 82 40 5f

- No.: 8955
- Timestamp: 20:44:37:390_1
- RFN: 6180
- Chip: 3584
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 8956
- Timestamp: 20:44:37:390_2
- RFN: 6180
- Chip: 4608
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 8961
- Timestamp: 20:44:37:408_1
- RFN: 6181
- Chip: 34560
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 8985
- Timestamp: 20:44:37:457_0
- RFN: 6186
- Chip: 25856
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001101011'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'F6670F2B2ED1B7C735876A710D7E26'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 59 1e f6 67 0f 2b 2e d1 b7 c7 35 87 6a 71 0d 7e 26

- No.: 8994
- Timestamp: 20:44:37:471_1
- RFN: 6188
- Chip: 3840
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 8995
- Timestamp: 20:44:37:471_2
- RFN: 6188
- Chip: 5376
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 8998
- Timestamp: 20:44:37:479_0
- RFN: 6188
- Chip: 34560
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001101001'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '9197C2605AA3BAC6E0E54F74D8B6B8'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 4d 1e 91 97 c2 60 5a a3 ba c6 e0 e5 4f 74 d8 b6 b8

- No.: 9015
- Timestamp: 20:44:37:506_3
- RFN: 6191
- Chip: 25344
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 9018
- Timestamp: 20:44:37:510_1
- RFN: 6192
- Chip: 512
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 9042
- Timestamp: 20:44:37:560_0
- RFN: 6197
- Chip: 2560
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001101100'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '50F7E730D2B7B8C6B5B893E8640F54'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 61 1e 50 f7 e7 30 d2 b7 b8 c6 b5 b8 93 e8 64 0f 54

- No.: 9051
- Timestamp: 20:44:37:574_1
- RFN: 6198
- Chip: 17664
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 9052
- Timestamp: 20:44:37:575_0
- RFN: 6198
- Chip: 18944
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 9055
- Timestamp: 20:44:37:582_0
- RFN: 6199
- Chip: 9728
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001101010'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = 'EC1B56DDB638F94C21FA991682405F'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 55 1e ec 1b 56 dd b6 38 f9 4c 21 fa 99 16 82 40 5f

- No.: 9072
- Timestamp: 20:44:37:613_0
- RFN: 6202
- Chip: 11520
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 9075
- Timestamp: 20:44:37:620_0
- RFN: 6203
- Chip: 3072
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001101011'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = 'F6670F2B2ED1B7C735876A710D7E26'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 5d 1e f6 67 0f 2b 2e d1 b7 c7 35 87 6a 71 0d 7e 26

- No.: 9092
- Timestamp: 20:44:37:647_3
- RFN: 6205
- Chip: 30464
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 9095
- Timestamp: 20:44:37:651_0
- RFN: 6206
- Chip: 5376
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 9119
- Timestamp: 20:44:37:698_0
- RFN: 6210
- Chip: 35584
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001101101'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'DDE36525D09D4375277A73A790C2B5'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 69 1e dd e3 65 25 d0 9d 43 75 27 7a 73 a7 90 c2 b5

- No.: 9128
- Timestamp: 20:44:37:716_0
- RFN: 6212
- Chip: 24576
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 9129
- Timestamp: 20:44:37:716_1
- RFN: 6212
- Chip: 25344
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 9132
- Timestamp: 20:44:37:723_0
- RFN: 6213
- Chip: 16128
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001101100'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '50F7E730D2B7B8C6B5B893E8640F54'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 65 1e 50 f7 e7 30 d2 b7 b8 c6 b5 b8 93 e8 64 0f 54

- No.: 9149
- Timestamp: 20:44:37:750_3
- RFN: 6216
- Chip: 4864
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 9152
- Timestamp: 20:44:37:754_1
- RFN: 6216
- Chip: 18688
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 9176
- Timestamp: 20:44:37:806_0
- RFN: 6221
- Chip: 23296
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001101110'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '1228515D7627058095422050080155'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 71 1e 12 28 51 5d 76 27 05 80 95 42 20 50 08 01 55

- No.: 9185
- Timestamp: 20:44:37:820_0
- RFN: 6222
- Chip: 38144
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 9186
- Timestamp: 20:44:37:820_1
- RFN: 6223
- Chip: 768
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 9191
- Timestamp: 20:44:37:841_1
- RFN: 6225
- Chip: 5120
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 9215
- Timestamp: 20:44:37:892_0
- RFN: 6230
- Chip: 8192
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001101111'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '777272F2E7B0C7E0CFE19A96E8E41A'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 79 1e 77 72 72 f2 e7 b0 c7 e0 cf e1 9a 96 e8 e4 1a

- No.: 9224
- Timestamp: 20:44:37:906_0
- RFN: 6231
- Chip: 24064
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 9225
- Timestamp: 20:44:37:906_1
- RFN: 6231
- Chip: 24832
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 9228
- Timestamp: 20:44:37:914_0
- RFN: 6232
- Chip: 15872
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001101101'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = 'DDE36525D09D4375277A73A790C2B5'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 6d 1e dd e3 65 25 d0 9d 43 75 27 7a 73 a7 90 c2 b5

- No.: 9245
- Timestamp: 20:44:37:941_1
- RFN: 6235
- Chip: 5120
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 9248
- Timestamp: 20:44:37:945_0
- RFN: 6235
- Chip: 19456
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 9272
- Timestamp: 20:44:37:997_0
- RFN: 6240
- Chip: 31232
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001110000'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '03AAC44A0BAB913D79D963DAC91E83'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 81 1e 03 aa c4 4a 0b ab 91 3d 79 d9 63 da c9 1e 83

- No.: 9281
- Timestamp: 20:44:38:011_1
- RFN: 6242
- Chip: 7936
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 9282
- Timestamp: 20:44:38:012_0
- RFN: 6242
- Chip: 8704
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 9285
- Timestamp: 20:44:38:019_0
- RFN: 6242
- Chip: 37632
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001101110'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '1228515D7627058095422050080155'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 75 1e 12 28 51 5d 76 27 05 80 95 42 20 50 08 01 55

- No.: 9302
- Timestamp: 20:44:38:048_1
- RFN: 6245
- Chip: 33536
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 9305
- Timestamp: 20:44:38:052_0
- RFN: 6246
- Chip: 9216
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 9329
- Timestamp: 20:44:38:103_0
- RFN: 6251
- Chip: 11520
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001110001'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '15288415FDCC9E165708D41DFC99E9'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 89 1e 15 28 84 15 fd cc 9e 16 57 08 d4 1d fc 99 e9

- No.: 9338
- Timestamp: 20:44:38:117_1
- RFN: 6252
- Chip: 29184
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 9339
- Timestamp: 20:44:38:118_0
- RFN: 6252
- Chip: 30208
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 9342
- Timestamp: 20:44:38:125_0
- RFN: 6253
- Chip: 20992
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001101111'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '777272F2E7B0C7E0CFE19A96E8E41A'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 7d 1e 77 72 72 f2 e7 b0 c7 e0 cf e1 9a 96 e8 e4 1a

- No.: 9359
- Timestamp: 20:44:38:155_3
- RFN: 6256
- Chip: 21248
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 9362
- Timestamp: 20:44:38:163_0
- RFN: 6257
- Chip: 12288
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001110000'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '03AAC44A0BAB913D79D963DAC91E83'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 85 1e 03 aa c4 4a 0b ab 91 3d 79 d9 63 da c9 1e 83

- No.: 9379
- Timestamp: 20:44:38:190_2
- RFN: 6260
- Chip: 1024
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 9382
- Timestamp: 20:44:38:194_0
- RFN: 6260
- Chip: 15104
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 9406
- Timestamp: 20:44:38:242_0
- RFN: 6265
- Chip: 8704
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001110010'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '6425FA33AD3B792685BF6CDB49217A'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 91 1e 64 25 fa 33 ad 3b 79 26 85 bf 6c db 49 21 7a

- No.: 9415
- Timestamp: 20:44:38:258_1
- RFN: 6266
- Chip: 33792
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 9416
- Timestamp: 20:44:38:259_0
- RFN: 6266
- Chip: 34560
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 9419
- Timestamp: 20:44:38:266_0
- RFN: 6267
- Chip: 26368
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001110001'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '15288415FDCC9E165708D41DFC99E9'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 8d 1e 15 28 84 15 fd cc 9e 16 57 08 d4 1d fc 99 e9

- No.: 9436
- Timestamp: 20:44:38:294_1
- RFN: 6270
- Chip: 17152
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 9439
- Timestamp: 20:44:38:297_1
- RFN: 6270
- Chip: 30976
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 9463
- Timestamp: 20:44:38:345_0
- RFN: 6275
- Chip: 23040
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001110011'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '8C41F56770D81C0355222FAE6E5B09'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 99 1e 8c 41 f5 67 70 d8 1c 03 55 22 2f ae 6e 5b 09

- No.: 9472
- Timestamp: 20:44:38:359_1
- RFN: 6277
- Chip: 512
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 9473
- Timestamp: 20:44:38:360_0
- RFN: 6277
- Chip: 1792
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 9478
- Timestamp: 20:44:38:378_1
- RFN: 6278
- Chip: 34816
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 9502
- Timestamp: 20:44:38:430_0
- RFN: 6283
- Chip: 37376
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001110100'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '2BD137D262F04D5E23052A2EFB1929'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 a1 1e 2b d1 37 d2 62 f0 4d 5e 23 05 2a 2e fb 19 29

- No.: 9511
- Timestamp: 20:44:38:444_0
- RFN: 6285
- Chip: 14336
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 9512
- Timestamp: 20:44:38:444_1
- RFN: 6285
- Chip: 15104
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 9515
- Timestamp: 20:44:38:451_0
- RFN: 6286
- Chip: 5632
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001110010'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '6425FA33AD3B792685BF6CDB49217A'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 95 1e 64 25 fa 33 ad 3b 79 26 85 bf 6c db 49 21 7a

- No.: 9532
- Timestamp: 20:44:38:480_1
- RFN: 6289
- Chip: 256
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 9535
- Timestamp: 20:44:38:483_1
- RFN: 6289
- Chip: 13824
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 9559
- Timestamp: 20:44:38:533_0
- RFN: 6294
- Chip: 14848
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001110101'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '7BD9368715823FACC4B5EDCE34F8B3'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 a9 1e 7b d9 36 87 15 82 3f ac c4 b5 ed ce 34 f8 b3

- No.: 9568
- Timestamp: 20:44:38:548_0
- RFN: 6295
- Chip: 31232
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 9569
- Timestamp: 20:44:38:548_1
- RFN: 6295
- Chip: 32768
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 9572
- Timestamp: 20:44:38:556_0
- RFN: 6296
- Chip: 23552
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001110011'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '8C41F56770D81C0355222FAE6E5B09'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 9d 1e 8c 41 f5 67 70 d8 1c 03 55 22 2f ae 6e 5b 09

- No.: 9589
- Timestamp: 20:44:38:586_1
- RFN: 6299
- Chip: 24320
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 9592
- Timestamp: 20:44:38:594_0
- RFN: 6300
- Chip: 16384
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001110100'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '2BD137D262F04D5E23052A2EFB1929'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 a5 1e 2b d1 37 d2 62 f0 4d 5e 23 05 2a 2e fb 19 29

- No.: 9609
- Timestamp: 20:44:38:620_3
- RFN: 6303
- Chip: 3840
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 9612
- Timestamp: 20:44:38:624_1
- RFN: 6303
- Chip: 17920
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 9636
- Timestamp: 20:44:38:673_0
- RFN: 6308
- Chip: 13056
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001110110'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'ED31D29D1628FBE6CF1E7CF34D21D0'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 b1 1e ed 31 d2 9d 16 28 fb e6 cf 1e 7c f3 4d 21 d0

- No.: 9645
- Timestamp: 20:44:38:689_1
- RFN: 6309
- Chip: 38144
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 9646
- Timestamp: 20:44:38:689_2
- RFN: 6310
- Chip: 768
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 9649
- Timestamp: 20:44:38:697_0
- RFN: 6310
- Chip: 31488
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001110101'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '7BD9368715823FACC4B5EDCE34F8B3'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 ad 1e 7b d9 36 87 15 82 3f ac c4 b5 ed ce 34 f8 b3

- No.: 9666
- Timestamp: 20:44:38:725_3
- RFN: 6313
- Chip: 20736
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 9669
- Timestamp: 20:44:38:729_1
- RFN: 6313
- Chip: 35072
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 9693
- Timestamp: 20:44:38:777_0
- RFN: 6318
- Chip: 27392
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001110111'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '37F8CC1E03007FF332D2E2E51A2904'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 b9 1e 37 f8 cc 1e 03 00 7f f3 32 d2 e2 e5 1a 29 04

- No.: 9702
- Timestamp: 20:44:38:792_1
- RFN: 6320
- Chip: 9472
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 9703
- Timestamp: 20:44:38:793_0
- RFN: 6320
- Chip: 11264
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 9708
- Timestamp: 20:44:38:812_1
- RFN: 6322
- Chip: 9728
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 9732
- Timestamp: 20:44:38:863_0
- RFN: 6327
- Chip: 11776
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001111000'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '2A0455F7672585C09FE99BC39F9668'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 c1 1e 2a 04 55 f7 67 25 85 c0 9f e9 9b c3 9f 96 68

- No.: 9741
- Timestamp: 20:44:38:877_0
- RFN: 6328
- Chip: 27904
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 9742
- Timestamp: 20:44:38:877_1
- RFN: 6328
- Chip: 28928
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 9745
- Timestamp: 20:44:38:885_0
- RFN: 6329
- Chip: 19456
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001110110'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = 'ED31D29D1628FBE6CF1E7CF34D21D0'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 b5 1e ed 31 d2 9d 16 28 fb e6 cf 1e 7c f3 4d 21 d0

- No.: 9762
- Timestamp: 20:44:38:912_0
- RFN: 6332
- Chip: 8960
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 9765
- Timestamp: 20:44:38:915_1
- RFN: 6332
- Chip: 22528
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 9789
- Timestamp: 20:44:38:966_0
- RFN: 6337
- Chip: 25344
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001111001'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'F14D748DEB6470A7EF3187C0CAB447'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 c9 1e f1 4d 74 8d eb 64 70 a7 ef 31 87 c0 ca b4 47

- No.: 9798
- Timestamp: 20:44:38:981_1
- RFN: 6339
- Chip: 7168
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 9799
- Timestamp: 20:44:38:981_2
- RFN: 6339
- Chip: 7936
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 9802
- Timestamp: 20:44:38:989_0
- RFN: 6340
- Chip: 1024
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001110111'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '37F8CC1E03007FF332D2E2E51A2904'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 bd 1e 37 f8 cc 1e 03 00 7f f3 32 d2 e2 e5 1a 29 04

- No.: 9819
- Timestamp: 20:44:39:019_3
- RFN: 6343
- Chip: 1280
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 9822
- Timestamp: 20:44:39:028_0
- RFN: 6343
- Chip: 32000
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001111000'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '2A0455F7672585C09FE99BC39F9668'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 c5 1e 2a 04 55 f7 67 25 85 c0 9f e9 9b c3 9f 96 68

- No.: 9839
- Timestamp: 20:44:39:055_3
- RFN: 6346
- Chip: 21248
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 9842
- Timestamp: 20:44:39:059_1
- RFN: 6346
- Chip: 35072
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 9866
- Timestamp: 20:44:39:109_0
- RFN: 6351
- Chip: 36608
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001111010'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '5F232F84C0B547758DC1CA9EE9B16D'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 d1 1e 5f 23 2f 84 c0 b5 47 75 8d c1 ca 9e e9 b1 6d

- No.: 9875
- Timestamp: 20:44:39:124_1
- RFN: 6353
- Chip: 16640
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 9876
- Timestamp: 20:44:39:124_2
- RFN: 6353
- Chip: 17664
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 9879
- Timestamp: 20:44:39:132_0
- RFN: 6354
- Chip: 8704
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001111001'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = 'F14D748DEB6470A7EF3187C0CAB447'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 cd 1e f1 4d 74 8d eb 64 70 a7 ef 31 87 c0 ca b4 47

- No.: 9896
- Timestamp: 20:44:39:160_0
- RFN: 6356
- Chip: 38144
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 9899
- Timestamp: 20:44:39:163_1
- RFN: 6357
- Chip: 13824
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 9923
- Timestamp: 20:44:39:211_0
- RFN: 6362
- Chip: 6144
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001111011'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '71D836ADBB6C71F29843F5322D0480'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 d9 1e 71 d8 36 ad bb 6c 71 f2 98 43 f5 32 2d 04 80

- No.: 9932
- Timestamp: 20:44:39:225_1
- RFN: 6363
- Chip: 22528
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 9933
- Timestamp: 20:44:39:226_0
- RFN: 6363
- Chip: 23552
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 9938
- Timestamp: 20:44:39:251_1
- RFN: 6366
- Chip: 7168
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 9962
- Timestamp: 20:44:39:302_0
- RFN: 6371
- Chip: 9216
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001111100'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'BFECCE1E565DA36F8E6B0ED4E21AFC'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 e1 1e bf ec ce 1e 56 5d a3 6f 8e 6b 0e d4 e2 1a fc

- No.: 9971
- Timestamp: 20:44:39:315_1
- RFN: 6372
- Chip: 24320
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 9972
- Timestamp: 20:44:39:316_0
- RFN: 6372
- Chip: 25600
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 9975
- Timestamp: 20:44:39:323_0
- RFN: 6373
- Chip: 16128
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001111010'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '5F232F84C0B547758DC1CA9EE9B16D'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 d5 1e 5f 23 2f 84 c0 b5 47 75 8d c1 ca 9e e9 b1 6d

- No.: 9992
- Timestamp: 20:44:39:352_1
- RFN: 6376
- Chip: 7168
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 9995
- Timestamp: 20:44:39:355_1
- RFN: 6376
- Chip: 21248
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 10019
- Timestamp: 20:44:39:406_0
- RFN: 6381
- Chip: 22784
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001111101'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '4CA1EFCE61A56F718D6B7127D0C81E'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 e9 1e 4c a1 ef ce 61 a5 6f 71 8d 6b 71 27 d0 c8 1e

- No.: 10028
- Timestamp: 20:44:39:420_0
- RFN: 6382
- Chip: 37376
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 10029
- Timestamp: 20:44:39:420_1
- RFN: 6383
- Chip: 0
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 10032
- Timestamp: 20:44:39:427_0
- RFN: 6383
- Chip: 28672
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001111011'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '71D836ADBB6C71F29843F5322D0480'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 dd 1e 71 d8 36 ad bb 6c 71 f2 98 43 f5 32 2d 04 80

- No.: 10049
- Timestamp: 20:44:39:456_3
- RFN: 6386
- Chip: 25600
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 10052
- Timestamp: 20:44:39:464_0
- RFN: 6387
- Chip: 15360
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001111100'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = 'BFECCE1E565DA36F8E6B0ED4E21AFC'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 e5 1e bf ec ce 1e 56 5d a3 6f 8e 6b 0e d4 e2 1a fc

- No.: 10069
- Timestamp: 20:44:39:490_2
- RFN: 6390
- Chip: 2048
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 10072
- Timestamp: 20:44:39:494_0
- RFN: 6390
- Chip: 15872
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 10096
- Timestamp: 20:44:39:539_0
- RFN: 6395
- Chip: 0
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001111110'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'A9BBC6CA4BA13A86EA4EF4E74F2185'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 f1 1e a9 bb c6 ca 4b a1 3a 86 ea 4e f4 e7 4f 21 85

- No.: 10105
- Timestamp: 20:44:39:556_0
- RFN: 6396
- Chip: 24832
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 10106
- Timestamp: 20:44:39:556_1
- RFN: 6396
- Chip: 25600
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 10109
- Timestamp: 20:44:39:563_0
- RFN: 6397
- Chip: 15104
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001111101'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '4CA1EFCE61A56F718D6B7127D0C81E'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 ed 1e 4c a1 ef ce 61 a5 6f 71 8d 6b 71 27 d0 c8 1e

- No.: 10126
- Timestamp: 20:44:39:590_1
- RFN: 6400
- Chip: 2048
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 10129
- Timestamp: 20:44:39:593_1
- RFN: 6400
- Chip: 14848
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 10154
- Timestamp: 20:44:39:641_0
- RFN: 6405
- Chip: 8704
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001111111'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '6A2450A2BAEC4E0B012A8440A01002'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 fd 1e 6a 24 50 a2 ba ec 4e 0b 01 2a 84 40 a0 10 02

- No.: 10163
- Timestamp: 20:44:39:656_1
- RFN: 6406
- Chip: 23296
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 10164
- Timestamp: 20:44:39:656_2
- RFN: 6406
- Chip: 24320
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 10169
- Timestamp: 20:44:39:679_1
- RFN: 6408
- Chip: 36352
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 10178
- Timestamp: 20:44:39:700_0
- RFN: 6410
- Chip: 38144
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 14
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 10179
- Timestamp: 20:44:39:700_1
- RFN: 6411
- Chip: 768
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 10182
- Timestamp: 20:44:39:707_0
- RFN: 6411
- Chip: 28416
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001111110'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = 'A9BBC6CA4BA13A86EA4EF4E74F2185'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 f5 1e a9 bb c6 ca 4b a1 3a 86 ea 4e f4 e7 4f 21 85

- No.: 10199
- Timestamp: 20:44:39:734_0
- RFN: 6414
- Chip: 15104
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 10202
- Timestamp: 20:44:39:737_1
- RFN: 6414
- Chip: 28160
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 10211
- Timestamp: 20:44:39:755_0
- RFN: 6416
- Chip: 18944
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 14
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 10212
- Timestamp: 20:44:39:755_1
- RFN: 6416
- Chip: 19712
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 10217
- Timestamp: 20:44:39:779_1
- RFN: 6418
- Chip: 36352
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 10226
- Timestamp: 20:44:39:801_1
- RFN: 6421
- Chip: 6656
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 14
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 10227
- Timestamp: 20:44:39:802_0
- RFN: 6421
- Chip: 7680
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 10230
- Timestamp: 20:44:39:816_0
- RFN: 6422
- Chip: 23040
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 5
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. STATUS_PDU
. . (DC_Field)dC_Field[1] = '0'B
. . (CtrlPDU_Type)type[3] = '000'B
. . SuperFields
. . (HexStringType)superFieldsAndPadRx[35] = '20800000000000000000000000000000000'H
. . (Padding)paddingTx[0] = -
- Constraint:
car_StatusInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 02 08 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00

- No.: 10232
- Timestamp: 20:44:39:820_0
- RFN: 6423
- Chip: 0
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 10235
- Timestamp: 20:44:39:826_0
- RFN: 6423
- Chip: 24832
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000001111111'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '6A2450A2BAEC4E0B012A8440A01002'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 83 fd 1e 6a 24 50 a2 ba ec 4e 0b 01 2a 84 40 a0 10 02

- No.: 10251
- Timestamp: 20:44:39:860_0
- RFN: 6427
- Chip: 2560
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: tc_7_2_3_14:lt_ChkPollBitAndStatus LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. STATUS_PDU
. . (DC_Field)dC_Field[1] = '0'B
. . (CtrlPDU_Type)type[3] = '000'B
. . SuperFields
. . . SUFI_WindowSize
. . . SUFI_List
. . . SUFI_RList
. . . SUFI_Bitmap
. . . SUFI_MRW
. . . SUFI_MRW_ACK
. . . SUFI_NoMore
. . . SUFI_Ack
. . . . (SUFI_Type)type[4] = '0010'B
. . . . (AM_SeqNum)lsn[12] = '000010000000'B
. . (HexStringType)superFieldsAndPadRx[-1] = -
. . (Padding)paddingTx[-1] = '0000000000000000000000000000000'H
- Constraint:
cas_StatusReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 02 08 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00

- No.: 10254
- Timestamp: 20:44:39:862_1
- RFN: 6427
- Chip: 9472
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 10257
- Timestamp: 20:44:39:865_1
- RFN: 6427
- Chip: 23040
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 10286
- Timestamp: 20:44:39:924_0
- RFN: 6433
- Chip: 20224
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000100000001'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'AAEEE4E5E5CF618FC19FC3352DD1C8'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 88 0d 1e aa ee e4 e5 e5 cf 61 8f c1 9f c3 35 2d d1 c8

- No.: 10295
- Timestamp: 20:44:39:938_0
- RFN: 6434
- Chip: 33792
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 10296
- Timestamp: 20:44:39:938_1
- RFN: 6434
- Chip: 34560
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 10301
- Timestamp: 20:44:39:958_1
- RFN: 6436
- Chip: 34560
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 10310
- Timestamp: 20:44:39:977_0
- RFN: 6438
- Chip: 26112
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 14
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 10311
- Timestamp: 20:44:39:977_1
- RFN: 6438
- Chip: 27136
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 10316
- Timestamp: 20:44:39:992_1
- RFN: 6440
- Chip: 8960
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 10325
- Timestamp: 20:44:40:010_0
- RFN: 6441
- Chip: 38144
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 14
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 10326
- Timestamp: 20:44:40:010_1
- RFN: 6442
- Chip: 512
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 10331
- Timestamp: 20:44:40:026_1
- RFN: 6443
- Chip: 24320
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 10340
- Timestamp: 20:44:40:046_0
- RFN: 6445
- Chip: 22528
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 14
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 10341
- Timestamp: 20:44:40:046_1
- RFN: 6445
- Chip: 23296
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 10346
- Timestamp: 20:44:40:079_0
- RFN: 6448
- Chip: 37120
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 5
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. STATUS_PDU
. . (DC_Field)dC_Field[1] = '0'B
. . (CtrlPDU_Type)type[3] = '000'B
. . SuperFields
. . (HexStringType)superFieldsAndPadRx[35] = '20800000000000000000000000000000000'H
. . (Padding)paddingTx[0] = -
- Constraint:
car_StatusInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 02 08 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00

- No.: 10348
- Timestamp: 20:44:40:083_0
- RFN: 6449
- Chip: 11776
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 10351
- Timestamp: 20:44:40:085_1
- RFN: 6449
- Chip: 21760
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 10377
- Timestamp: 20:44:40:135_0
- RFN: 6454
- Chip: 22272
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000010000000'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'AAEEE4E5E5CF618FC19FC3352DD1C8'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 84 01 1e aa ee e4 e5 e5 cf 61 8f c1 9f c3 35 2d d1 c8

- No.: 10386
- Timestamp: 20:44:40:149_0
- RFN: 6455
- Chip: 35840
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 12
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 10387
- Timestamp: 20:44:40:149_1
- RFN: 6455
- Chip: 36608
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 10392
- Timestamp: 20:44:40:170_1
- RFN: 6458
- Chip: 2816
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 10400
- Timestamp: 20:44:40:185_1
- RFN: 6459
- Chip: 22528
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 14
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 10401
- Timestamp: 20:44:40:185_2
- RFN: 6459
- Chip: 23296
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 10406
- Timestamp: 20:44:40:193_1
- RFN: 6460
- Chip: 13568
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 10414
- Timestamp: 20:44:40:207_1
- RFN: 6461
- Chip: 31232
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 14
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 10415
- Timestamp: 20:44:40:208_0
- RFN: 6461
- Chip: 32256
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 10420
- Timestamp: 20:44:40:226_1
- RFN: 6463
- Chip: 26624
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 10428
- Timestamp: 20:44:40:241_1
- RFN: 6465
- Chip: 7424
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 14
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 10429
- Timestamp: 20:44:40:241_2
- RFN: 6465
- Chip: 8192
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 10434
- Timestamp: 20:44:40:259_1
- RFN: 6467
- Chip: 0
- Event: Timeout
- Source: tc_7_2_3_14:lt_TxAndRx LINE 7
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 10442
- Timestamp: 20:44:40:274_1
- RFN: 6468
- Chip: 19712
- Event: Start Timer
- Source: tc_7_2_3_14:lt_TxAndRx LINE 14
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 10443
- Timestamp: 20:44:40:274_2
- RFN: 6468
- Chip: 20480
- Event: Repeat
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 10448
- Timestamp: 20:44:40:295_0
- RFN: 6470
- Chip: 19712
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_14:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000010000000'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = 'AAEEE4E5E5CF618FC19FC3352DD1C8'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 84 05 1e aa ee e4 e5 e5 cf 61 8f c1 9f c3 35 2d d1 c8

- No.: 10466
- Timestamp: 20:44:40:323_1
- RFN: 6473
- Chip: 12800
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 8
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 10468
- Timestamp: 20:44:40:327_0
- RFN: 6473
- Chip: 26880
- Event: Cancel Timer
- Source: tc_7_2_3_14:lt_CtrlRxWindowTest LINE 9
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 10472
- Timestamp: 20:44:40:335_0
- RFN: 6474
- Chip: 21248
- Event: Send
- PCO: Dc
- Message: RRC_DataReq
- Source: ts_TC_OpenUE_TestLoop LINE 6
- Message Structure:
RRC_DataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[-1] = -
. (SapId)sapId[1] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. OPENUETESTLOOP
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)tCProtocolDiscriminator[4] = '1111'B
. . (MsgType)msgType[8] = '01000010'B
- Constraint:
ca_PS_DataReq
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 0f 42

- No.: 10473
- Timestamp: 20:44:40:336_0
- RFN: 6474
- Chip: 25344
- Event: Start Timer
- Source: ts_TC_OpenUE_TestLoop LINE 6
- Message Structure:
no details available
- Constraint:
t_Dly (5000 Ms)
- BinaryMessage:

- No.: 10477
- Timestamp: 20:44:40:614_0
- RFN: 6502
- Chip: 14080
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_TC_OpenUE_TestLoop LINE 7
- Message Structure:
RRC_DataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. (START_Value)start[0] = -
. OPENUETESTLOOPCOMPLETE
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)tCProtocolDiscriminator[4] = '1111'B
. . (MsgType)msgType[8] = '01000011'B
- Constraint:
car_PS_UplinkDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 0f 43

- No.: 10478
- Timestamp: 20:44:40:615_0
- RFN: 6502
- Chip: 17664
- Event: Cancel Timer
- Source: ts_TC_OpenUE_TestLoop LINE 7
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 10479
- Timestamp: 20:44:40:615_1
- RFN: 6502
- Chip: 18688
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_TC_OpenUE_TestLoop LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 10491
- Timestamp: 20:44:40:636_0
- RFN: 6504
- Chip: 24576
- Event: Send
- PCO: Dc
- Message: RRC_DataReq
- Source: ts_TC_DeactivateRB_TestMode LINE 6
- Message Structure:
RRC_DataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[-1] = -
. (SapId)sapId[1] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. DEACTIVATERBTESTMODE
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)tCProtocolDiscriminator[4] = '1111'B
. . (MsgType)msgType[8] = '01000110'B
- Constraint:
ca_PS_DataReq
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 0f 46

- No.: 10492
- Timestamp: 20:44:40:645_0
- RFN: 6505
- Chip: 21504
- Event: Start Timer
- Source: ts_TC_DeactivateRB_TestMode LINE 6
- Message Structure:
no details available
- Constraint:
t_Dly (5000 Ms)
- BinaryMessage:

- No.: 10496
- Timestamp: 20:44:40:931_0
- RFN: 6534
- Chip: 4864
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_TC_DeactivateRB_TestMode LINE 7
- Message Structure:
RRC_DataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. (START_Value)start[0] = -
. DEACTIVATERBTESTMODECOMPLETE
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)tCProtocolDiscriminator[4] = '1111'B
. . (MsgType)msgType[8] = '01000111'B
- Constraint:
car_PS_UplinkDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 0f 47

- No.: 10497
- Timestamp: 20:44:40:932_0
- RFN: 6534
- Chip: 8192
- Event: Cancel Timer
- Source: ts_TC_DeactivateRB_TestMode LINE 7
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 10498
- Timestamp: 20:44:40:932_1
- RFN: 6534
- Chip: 8960
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_TC_DeactivateRB_TestMode LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 10510
- Timestamp: 20:44:40:940_0
- RFN: 6535
- Chip: 512
- Event: Send
- PCO: UM
- Message: RLC_UM_DATA_REQ
- Source: po_ConnectionAndSS_Rel:lt_Send_RRC_ConnectionRelease LINE 8
- Message Structure:
RLC_UM_DATA_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. uM_message
. . DL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00000000000000000000000000000000"
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . DL_DCCH_MessageType
. . . . RRCConnectionRelease
. . . . . r3
. . . . . . RRCConnectionRelease_r3_IEs
. . . . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . . . (IntegerType)n_308 = 1
. . . . . . . (ReleaseCause)releaseCause = 0
. . . . . . . Rplmn_Information
. . . . . . laterNonCriticalExtensions
. (BooleanType)specialLI = FALSE
- Constraint:
cas_RRC_ConnRelDCCH
- BinaryMessage:
30 10 02 01 ff 02 01 01 80 00 00 00 03 c8 00 01 01 00

- No.: 10514
- Timestamp: 20:44:41:173_0
- RFN: 6558
- Chip: 14080
- Event: Receive
- PCO: UM
- Message: RLC_UM_DATA_IND
- Source: po_ConnectionAndSS_Rel:lt_Send_RRC_ConnectionRelease LINE 9
- Message Structure:
RLC_UM_DATA_IND
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. IntegrityResult
. uM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "10110011101011111111101100111000"
. . . . (IntegerType)rrc_MessageSequenceNumber = 1
. . . UL_DCCH_MessageType
. . . . RRCConnectionReleaseComplete
. . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . FailureCauseWithProtErr
. . . . . laterNonCriticalExtensions
. . . . . . (BitStringType)rrcConnectionReleaseComplete_r3_add_ext = 0
. . . . . . nonCriticalExtensions
- Constraint:
car_RRC_ConnRelCmplUM
- BinaryMessage:
30 0c 02 01 ff 02 01 01 d9 d7 fd 9c 0c 40

- No.: 10515
- Timestamp: 20:44:41:174_0
- RFN: 6558
- Chip: 17408
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: po_ConnectionAndSS_Rel:lt_Send_RRC_ConnectionRelease LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 10518
- Timestamp: 20:44:41:175_1
- RFN: 6558
- Chip: 22272
- Event: Start Timer
- Source: po_ConnectionAndSS_Rel:lt_RptRcvConnRel LINE 1
- Message Structure:
no details available
- Constraint:
t_Dly (5000 Ms)
- BinaryMessage:

- No.: 10522
- Timestamp: 20:44:41:332_0
- RFN: 6574
- Chip: 7680
- Event: Receive
- PCO: UM
- Message: RLC_UM_DATA_IND
- Source: po_ConnectionAndSS_Rel:lt_RptRcvConnRel LINE 4
- Message Structure:
RLC_UM_DATA_IND
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. IntegrityResult
. uM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00111001011111110001011000001001"
. . . . (IntegerType)rrc_MessageSequenceNumber = 2
. . . UL_DCCH_MessageType
. . . . RRCConnectionReleaseComplete
. . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . FailureCauseWithProtErr
. . . . . laterNonCriticalExtensions
. . . . . . (BitStringType)rrcConnectionReleaseComplete_r3_add_ext = 0
. . . . . . nonCriticalExtensions
- Constraint:
car_RRC_ConnRelCmplUM
- BinaryMessage:
30 0c 02 01 ff 02 01 01 9c bf 8b 04 94 40

- No.: 10523
- Timestamp: 20:44:41:333_0
- RFN: 6574
- Chip: 11776
- Event: Cancel Timer
- Source: po_ConnectionAndSS_Rel:lt_RptRcvConnRel LINE 4
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 10524
- Timestamp: 20:44:41:333_1
- RFN: 6574
- Chip: 12800
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: po_ConnectionAndSS_Rel:lt_RptRcvConnRel LINE 4
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 10540
- Timestamp: 20:44:41:389_0
- RFN: 6579
- Chip: 34816
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 01 0a 01 00 05 00

- No.: 10544
- Timestamp: 20:44:41:400_0
- RFN: 6581
- Chip: 512
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 10547
- Timestamp: 20:44:41:403_0
- RFN: 6581
- Chip: 12032
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 02 0a 01 00 05 00

- No.: 10551
- Timestamp: 20:44:41:410_0
- RFN: 6582
- Chip: 3328
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 10554
- Timestamp: 20:44:41:413_0
- RFN: 6582
- Chip: 14592
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 03 0a 01 00 05 00

- No.: 10558
- Timestamp: 20:44:41:420_0
- RFN: 6583
- Chip: 3584
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 10561
- Timestamp: 20:44:41:423_0
- RFN: 6583
- Chip: 14592
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 04 0a 01 00 05 00

- No.: 10565
- Timestamp: 20:44:41:431_0
- RFN: 6584
- Chip: 5888
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 10571
- Timestamp: 20:44:41:436_0
- RFN: 6584
- Chip: 25856
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = -12
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 f4 0a 01 00 05 00

- No.: 10573
- Timestamp: 20:44:41:442_0
- RFN: 6585
- Chip: 9984
- Event: Receive
- PCO: CPHY
- Message: CPHY_Out_of_Sync_IND
- Source: SS_Def LINE 5
- Message Structure:
CPHY_Out_of_Sync_IND
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_OutOfSyncInd
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 10574
- Timestamp: 20:44:41:443_0
- RFN: 6585
- Chip: 13824
- Event: Default
- Source: SS_Def LINE 0
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 10575
- Timestamp: 20:44:41:443_1
- RFN: 6585
- Chip: 14592
- Event: Default
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 10577
- Timestamp: 20:44:41:445_0
- RFN: 6585
- Chip: 21760
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = -12
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 f4

- No.: 10581
- Timestamp: 20:44:41:454_0
- RFN: 6586
- Chip: 18176
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_CMAC_Rel LINE 1
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
. (RatType)ratType = 0
. configMessage
- Constraint:
cas_MAC_Rel
- BinaryMessage:
30 0b 02 01 ff 02 01 1a 0a 01 00 05 00

- No.: 10585
- Timestamp: 20:44:41:462_0
- RFN: 6587
- Chip: 10496
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_CMAC_Rel LINE 2
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 1a

- No.: 10588
- Timestamp: 20:44:41:469_0
- RFN: 6587
- Chip: 36608
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_CMAC_Rel LINE 1
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
. (RatType)ratType = 0
. configMessage
- Constraint:
cas_MAC_Rel
- BinaryMessage:
30 0b 02 01 ff 02 01 14 0a 01 00 05 00

- No.: 10592
- Timestamp: 20:44:41:476_0
- RFN: 6588
- Chip: 27904
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_CMAC_Rel LINE 2
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 14

- No.: 10595
- Timestamp: 20:44:41:487_0
- RFN: 6589
- Chip: 28416
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Release_REQ
- Source: ts_CPHY_TrChRel LINE 1
- Message Structure:
CPHY_TrCH_Release_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
ca_PHY_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 1a

- No.: 10599
- Timestamp: 20:44:41:495_0
- RFN: 6590
- Chip: 22784
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Release_CNF
- Source: ts_CPHY_TrChRel LINE 2
- Message Structure:
CPHY_TrCH_Release_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
ca_PHY_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 1a

- No.: 10602
- Timestamp: 20:44:41:498_0
- RFN: 6590
- Chip: 33280
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Release_REQ
- Source: ts_CPHY_TrChRel LINE 1
- Message Structure:
CPHY_TrCH_Release_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_PHY_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 10606
- Timestamp: 20:44:41:526_0
- RFN: 6593
- Chip: 28160
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Release_CNF
- Source: ts_CPHY_TrChRel LINE 2
- Message Structure:
CPHY_TrCH_Release_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_PHY_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 10609
- Timestamp: 20:44:41:530_0
- RFN: 6594
- Chip: 1536
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 1a

- No.: 10613
- Timestamp: 20:44:41:540_0
- RFN: 6594
- Chip: 37632
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 1a

- No.: 10616
- Timestamp: 20:44:41:543_0
- RFN: 6595
- Chip: 9984
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 10620
- Timestamp: 20:44:41:568_0
- RFN: 6597
- Chip: 32768
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 10625
- Timestamp: 20:44:41:594_0
- RFN: 6600
- Chip: 14336
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 00 02 01 00 0a 01 00 05 00

- No.: 10629
- Timestamp: 20:44:41:599_0
- RFN: 6600
- Chip: 35584
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 00

- No.: 10632
- Timestamp: 20:44:41:603_0
- RFN: 6601
- Chip: 13312
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_CMAC_Rel LINE 1
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 8
. (RatType)ratType = 0
. configMessage
- Constraint:
cas_MAC_Rel
- BinaryMessage:
30 0b 02 01 00 02 01 08 0a 01 00 05 00

- No.: 10636
- Timestamp: 20:44:41:608_0
- RFN: 6601
- Chip: 32512
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_CMAC_Rel LINE 2
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 8
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 08

- No.: 10639
- Timestamp: 20:44:41:611_0
- RFN: 6602
- Chip: 4608
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Release_REQ
- Source: ts_CPHY_TrChRel LINE 1
- Message Structure:
CPHY_TrCH_Release_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 8
- Constraint:
ca_PHY_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 08

- No.: 10643
- Timestamp: 20:44:41:638_0
- RFN: 6604
- Chip: 30464
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Release_CNF
- Source: ts_CPHY_TrChRel LINE 2
- Message Structure:
CPHY_TrCH_Release_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 8
- Constraint:
ca_PHY_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 08

- No.: 10646
- Timestamp: 20:44:41:640_0
- RFN: 6605
- Chip: 2560
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 7
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 07

- No.: 10650
- Timestamp: 20:44:41:647_0
- RFN: 6605
- Chip: 29696
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 7
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 07

- No.: 10653
- Timestamp: 20:44:41:650_0
- RFN: 6606
- Chip: 1792
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 8
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 08

- No.: 10657
- Timestamp: 20:44:41:678_0
- RFN: 6608
- Chip: 30976
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 8
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 08

- No.: 10660
- Timestamp: 20:44:41:697_0
- RFN: 6610
- Chip: 30464
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -2
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 00 02 01 fe 0a 01 00 05 00

- No.: 10664
- Timestamp: 20:44:41:746_0
- RFN: 6615
- Chip: 24064
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 fe

- No.: 10667
- Timestamp: 20:44:41:791_0
- RFN: 6620
- Chip: 7424
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_CMAC_Rel LINE 1
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 5
. (RatType)ratType = 0
. configMessage
- Constraint:
cas_MAC_Rel
- BinaryMessage:
30 0b 02 01 00 02 01 05 0a 01 00 05 00

- No.: 10671
- Timestamp: 20:44:41:797_0
- RFN: 6620
- Chip: 30976
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_CMAC_Rel LINE 2
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 5
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 05

- No.: 10674
- Timestamp: 20:44:41:800_0
- RFN: 6621
- Chip: 2560
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Release_REQ
- Source: ts_CPHY_TrChRel LINE 1
- Message Structure:
CPHY_TrCH_Release_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 5
- Constraint:
ca_PHY_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 05

- No.: 10678
- Timestamp: 20:44:41:807_0
- RFN: 6621
- Chip: 29696
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Release_CNF
- Source: ts_CPHY_TrChRel LINE 2
- Message Structure:
CPHY_TrCH_Release_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 5
- Constraint:
ca_PHY_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 05

- No.: 10681
- Timestamp: 20:44:41:810_0
- RFN: 6622
- Chip: 1792
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 6
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 06

- No.: 10685
- Timestamp: 20:44:41:818_0
- RFN: 6622
- Chip: 33792
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 6
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 06

- No.: 10688
- Timestamp: 20:44:41:827_0
- RFN: 6623
- Chip: 29696
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 5
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 05

- No.: 10692
- Timestamp: 20:44:41:850_0
- RFN: 6626
- Chip: 1536
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 5
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 05

- No.: 10697
- Timestamp: 20:44:41:854_0
- RFN: 6626
- Chip: 13824
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 00 02 01 ff 0a 01 00 05 00

- No.: 10701
- Timestamp: 20:44:41:897_0
- RFN: 6630
- Chip: 28160
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 10704
- Timestamp: 20:44:41:901_0
- RFN: 6631
- Chip: 2816
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_CMAC_Rel LINE 1
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 4
. (RatType)ratType = 0
. configMessage
- Constraint:
cas_MAC_Rel
- BinaryMessage:
30 0b 02 01 00 02 01 04 0a 01 00 05 00

- No.: 10708
- Timestamp: 20:44:41:907_0
- RFN: 6631
- Chip: 27648
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_CMAC_Rel LINE 2
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 4
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 04

- No.: 10711
- Timestamp: 20:44:41:914_0
- RFN: 6632
- Chip: 16640
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Release_REQ
- Source: ts_CPHY_TrChRel LINE 1
- Message Structure:
CPHY_TrCH_Release_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 4
- Constraint:
ca_PHY_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 04

- No.: 10715
- Timestamp: 20:44:41:920_0
- RFN: 6633
- Chip: 1536
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Release_CNF
- Source: ts_CPHY_TrChRel LINE 2
- Message Structure:
CPHY_TrCH_Release_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 4
- Constraint:
ca_PHY_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 04

- No.: 10718
- Timestamp: 20:44:41:923_0
- RFN: 6633
- Chip: 12544
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 2
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 02

- No.: 10722
- Timestamp: 20:44:41:928_0
- RFN: 6633
- Chip: 34048
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 2
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 02

- No.: 10725
- Timestamp: 20:44:41:931_0
- RFN: 6634
- Chip: 5888
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 1
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 01

- No.: 10729
- Timestamp: 20:44:41:937_0
- RFN: 6634
- Chip: 26880
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 1
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 01

- No.: 10732
- Timestamp: 20:44:41:939_0
- RFN: 6634
- Chip: 37376
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 4
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 04

- No.: 10736
- Timestamp: 20:44:41:947_0
- RFN: 6635
- Chip: 26880
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 4
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 04

- No.: 10739
- Timestamp: 20:44:41:949_0
- RFN: 6635
- Chip: 36352
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 0
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 00

- No.: 10743
- Timestamp: 20:44:41:956_0
- RFN: 6636
- Chip: 24832
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 0
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 00

- No.: 10760
- Timestamp: 20:44:41:971_0
- RFN: 6638
- Chip: 4608
- Event: Log
- PCO: VERDICT
- Message: PASS
- Source: tc_7_2_3_14 LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage: