- No.: 2
- Timestamp: 20:48:23:794_0
- RFN: 4066
- Chip: 13312
- Event: Start Timer
- Source: tc_7_2_3_18 LINE 1
- Message Structure:
no details available
- Constraint:
t_Guard (300 Sec)
- BinaryMessage:

- No.: 88
- Timestamp: 20:48:23:827_0
- RFN: 4069
- Chip: 21760
- Event: Send
- PCO: Ut
- Message: MMI_CmdReq
- Source: ts_MMI_UE_SwitchOff LINE 1
- Message Structure:
MMI_CmdReq
. (IA5StringType)cmd[-1] = "Please switch off the UE"
- Constraint:
ca_MMI_CmdReq
- BinaryMessage:
50 6c 65 61 73 65 20 73 77 69 74 63 68 20 6f 66 66 20 20 74 68 65 20 55 45

- No.: 92
- Timestamp: 20:48:26:018_0
- RFN: 4288
- Chip: 26368
- Event: Receive
- PCO: Ut
- Message: MMI_CmdCnf
- Source: ts_MMI_UE_SwitchOff LINE 2
- Message Structure:
MMI_CmdCnf
. (BooleanType)result = TRUE
. (IA5StringType)resultString[6] = " OK "
- Constraint:
ca_MMI_CmdCnf
- BinaryMessage:
80 0d 0a 4f 4b 0d 0a

- No.: 96
- Timestamp: 20:48:26:021_0
- RFN: 4288
- Chip: 36352
- Event: Send
- PCO: CPHY
- Message: CPHY_Ini_REQ
- Source: ts_SS_CellCfg:lt_CelllsAlreadyStarted LINE 5
- Message Structure:
CPHY_Ini_REQ
. (CPHY_Ini_REQ)CPHY_Ini_REQ = 0
- Constraint:
cas_InitReqDef
- BinaryMessage:
0a 01 00

- No.: 100
- Timestamp: 20:48:28:057_0
- RFN: 10
- Chip: 14848
- Event: Receive
- PCO: CPHY
- Message: CPHY_Ini_CNF
- Source: ts_SS_CellCfg:lt_CelllsAlreadyStarted LINE 6
- Message Structure:
CPHY_Ini_CNF
- Constraint:
car_IniCnf
- BinaryMessage:
30 02 05 00

- No.: 104
- Timestamp: 20:48:28:059_0
- RFN: 10
- Chip: 25600
- Event: Send
- PCO: CPHY
- Message: CPHY_Cell_Config_REQ
- Source: ts_SS_CellCfg LINE 6
- Message Structure:
CPHY_Cell_Config_REQ
. (IntegerType)cellId = 0
. (IntegerType)tcell = 0
. (IntegerType)sfnOffset = 0
. FrequencyInfo
. . modeSpecificInfo
. . . FrequencyInfoFDD
. . . . (IntegerType)uarfcn_UL = -
. . . . (IntegerType)uarfcn_DL = 10700
. (IntegerType)primaryScramblingCode_SS = 100
. CellTxPowerLevel
. (IntegerType)dLTxAttenuationLevel = 0
- Constraint:
ca_CellCfgReq
- BinaryMessage:
30 19 02 01 00 02 01 00 02 01 00 30 06 30 04 02 02 29 cc 02 01 64 05 00 02 01 00

- No.: 108
- Timestamp: 20:48:28:971_0
- RFN: 101
- Chip: 31232
- Event: Receive
- PCO: CPHY
- Message: CPHY_Cell_Config_CNF
- Source: ts_SS_CellCfg LINE 7
- Message Structure:
CPHY_Cell_Config_CNF
. (IntegerType)cellId = 0
- Constraint:
ca_CellCfgCnf
- BinaryMessage:
30 03 02 01 00

- No.: 120
- Timestamp: 20:48:28:977_0
- RFN: 102
- Chip: 16896
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 3
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 0
. (RatType)ratType = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . PrimaryCPICHInfo
. . . . (IntegerType)dl_TxPower_PCPICH = -60
. . . . (BooleanType)txdiversityIndicator = FALSE
- Constraint:
ca_pCPICH_Info
- BinaryMessage:
30 13 02 01 00 02 01 00 0a 01 00 30 08 30 06 02 01 c4 01 01 00

- No.: 124
- Timestamp: 20:48:28:983_0
- RFN: 103
- Chip: 256
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 4
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 0
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 00

- No.: 125
- Timestamp: 20:48:28:986_0
- RFN: 103
- Chip: 12800
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 5
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 1
. (RatType)ratType = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . PrimarySCHInfo
. . . . (BooleanType)tstdIndicator = FALSE
. . . . (IntegerType)dl_TxPower = -5
- Constraint:
ca_pSCH_Info
- BinaryMessage:
30 13 02 01 00 02 01 01 0a 01 00 30 08 30 06 01 01 00 02 01 fb

- No.: 129
- Timestamp: 20:48:28:991_0
- RFN: 103
- Chip: 32000
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 6
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 1
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 01

- No.: 130
- Timestamp: 20:48:28:994_0
- RFN: 104
- Chip: 6656
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 7
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 2
. (RatType)ratType = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . SecondarySCHInfo
. . . . (BooleanType)tstdIndicator = FALSE
. . . . (IntegerType)dl_TxPower = -5
- Constraint:
ca_sSCH_Info
- BinaryMessage:
30 13 02 01 00 02 01 02 0a 01 00 30 08 30 06 01 01 00 02 01 fb

- No.: 134
- Timestamp: 20:48:29:133_0
- RFN: 118
- Chip: 2304
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 8
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 2
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 02

- No.: 135
- Timestamp: 20:48:29:136_0
- RFN: 118
- Chip: 15616
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 9
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 4
. (RatType)ratType = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . PrimaryCCPCHInfo
. . . . (BooleanType)sttd_Indicator = FALSE
. . . . (IntegerType)dl_TxPower = -2
- Constraint:
ca_pCCPCH_Info
- BinaryMessage:
30 13 02 01 00 02 01 04 0a 01 00 30 08 30 06 01 01 00 02 01 fe

- No.: 139
- Timestamp: 20:48:29:143_0
- RFN: 119
- Chip: 3328
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 10
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 4
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 04

- No.: 140
- Timestamp: 20:48:29:155_0
- RFN: 120
- Chip: 7424
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Config_REQ
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 11
- Message Structure:
CPHY_TrCH_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 4
. (RatType)ratType = 0
. CphyTrchConfigReq
. . SS_ActivationTime
. . ulconnectedTrCHList
. . TFCS
. . dlconnectedTrCHList
. . . CphyTrchConfigReq_setseq_1
. . . . (IntegerType)trchid = 11
. . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 2
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 246
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional = 0
. . . . . . (IntegerType)rateMatchingAttribute = 1
. . . . . . (CRC_Size)crc_Size = 3
. . TFCS
. . . ExplicitTFCS_Configuration
. . . . TFCS_ReconfAdd
. . . . . ctfcSize
. . . . . . ctfc2Bit
. . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . (IntegerType)ctfc2 = 0
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . fdd
. . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 11
. . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
- Constraint:
ca_BCH_InfoActNow
- BinaryMessage:
30 4c 02 01 00 02 01 04 0a 01 00 30 41 05 00 30 23 30 21 02 01 0b 0a 01 02 30 19 30 0c 30 0a 02 02 00 f6 30 02 05 00 05 00 30 09 0a 01 00 02 01 01 0a 01 03 30 18 30 30 15 30 13 02 01 00 30 0e 30 0c 30 30 03 02 01 0b 02 01 0f 02 01 00

- No.: 144
- Timestamp: 20:48:29:163_0
- RFN: 120
- Chip: 35840
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Config_CNF
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 12
- Message Structure:
CPHY_TrCH_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 4
- Constraint:
ca_TrChCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 04

- No.: 145
- Timestamp: 20:48:29:178_0
- RFN: 122
- Chip: 19200
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 13
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 4
. (RatType)ratType = 0
. configMessage
. . CmacConfigReq
. . . SS_ActivationTime
. . . UE_Info
. . . . U_RNTI
. . . . (BitStringType)c_RNTI[16] = -
. . . TrCHInfo
. . . . ulconnectedTrCHList
. . . . TFCS
. . . . dlconnectedTrCHList
. . . . . TrCHInfo_setseq_1
. . . . . . (IntegerType)trchid = 11
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 246
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional = 0
. . . . . . . . (IntegerType)rateMatchingAttribute = 1
. . . . . . . . (CRC_Size)crc_Size = 3
. . . . TFCS
. . . . . ExplicitTFCS_Configuration
. . . . . . TFCS_ReconfAdd
. . . . . . . ctfcSize
. . . . . . . . ctfc2Bit
. . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . (IntegerType)ctfc2 = 0
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 11
. . . . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . TrCH_LogCHMappingList1
. . . . ulconnectedTrCHList
. . . . dlconnectedTrCHList
. . . . . TrCH_LogCHMappingList1_setseq_1
. . . . . . (IntegerType)trchid = 11
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 2
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 0
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 1
. . . . . . . . (IntegerType)rB_Identity = -1
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_CMAC_CfgInfo
- BinaryMessage:
30 70 02 01 00 02 01 04 0a 01 00 30 65 05 00 30 00 30 3c 30 20 30 1e 02 01 0b 30 19 30 0c 30 0a 02 02 00 f6 30 02 05 00 05 00 30 09 0a 01 00 02 01 01 0a 01 03 30 18 30 30 15 30 13 02 01 00 30 0e 30 0c 30 30 03 02 01 0b 02 01 0f 02 01 00 30 21 30 1f 30 1d 02 01 0b 30 18 30 16 30 11 0a 01 00 0a 01 02 02 01 01 0a 01 00 05 00 02 01 01 02 01 ff

- No.: 149
- Timestamp: 20:48:29:189_0
- RFN: 123
- Chip: 22784
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 14
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 4
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 04

- No.: 157
- Timestamp: 20:48:29:195_0
- RFN: 124
- Chip: 7424
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_PCH_FACH_CCCH_Cfg LINE 3
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 5
. (RatType)ratType = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . SecondaryCCPCHInfo
. . . . (IntegerType)scramblingCode = 0
. . . . SF256_AndCodeNumber
. . . . . (IntegerType)sf64 = 1
. . . . (IntegerType)sCCPCHSlotFormat = 8
. . . . (IntegerType)timingOffset = 0
. . . . (PositionFixedOrFlexible)positionFixedOrFlexible = 1
. . . . (BooleanType)sttd_Indicator = FALSE
. . . . (IntegerType)dl_TxPower = -2
. . . . (IntegerType)powerOffsetOfTFCI_PO1 = 6
. . . . (IntegerType)powerOffsetOfPILOT_PO3 = 6
- Constraint:
ca_sCCPCH_Info
- BinaryMessage:
30 28 02 01 00 02 01 05 0a 01 00 30 1d 30 1b 02 01 00 02 01 01 02 01 08 02 01 00 0a 01 01 01 01 00 02 01 fe 02 01 06 02 01 06

- No.: 161
- Timestamp: 20:48:29:202_0
- RFN: 124
- Chip: 34304
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_PCH_FACH_CCCH_Cfg LINE 4
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 5
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 05

- No.: 162
- Timestamp: 20:48:29:227_0
- RFN: 127
- Chip: 16896
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Config_REQ
- Source: ts_SS_PCH_FACH_CCCH_Cfg LINE 5
- Message Structure:
CPHY_TrCH_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 5
. (RatType)ratType = 0
. CphyTrchConfigReq
. . SS_ActivationTime
. . ulconnectedTrCHList
. . TFCS
. . dlconnectedTrCHList
. . . CphyTrchConfigReq_setseq_1
. . . . (IntegerType)trchid = 12
. . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 3
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 240
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional = 0
. . . . . . (IntegerType)rateMatchingAttribute = 230
. . . . . . (CRC_Size)crc_Size = 3
. . . CphyTrchConfigReq_setseq_1
. . . . (IntegerType)trchid = 13
. . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 1
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 168
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . (IntegerType)small = 2
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional = 0
. . . . . . (IntegerType)rateMatchingAttribute = 220
. . . . . . (CRC_Size)crc_Size = 3
. . . CphyTrchConfigReq_setseq_1
. . . . (IntegerType)trchid = 14
. . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 1
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 360
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . (IntegerType)rateMatchingAttribute = 130
. . . . . . (CRC_Size)crc_Size = 3
. . TFCS
. . . ExplicitTFCS_Configuration
. . . . TFCS_ReconfAdd
. . . . . ctfcSize
. . . . . . ctfc4Bit
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 0
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 1
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 2
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 3
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 4
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 5
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 6
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 8
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . fdd
. . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 11
. . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
- Constraint:
ca_PCH_2_FACH_InfoActNow
- BinaryMessage:
30 81 e4 02 01 00 02 01 05 0a 01 00 30 81 d8 05 00 30 74 30 24 02 01 0c 0a 01 03 30 1c 30 0e 30 0c 02 02 00 f0 30 04 05 00 05 00 05 00 30 0a 0a 01 00 02 02 00 e6 0a 01 03 30 27 02 01 0d 0a 01 01 30 1f 30 11 30 0f 02 02 00 a8 30 07 05 00 05 00 02 01 02 05 00 30 0a 0a 01 00 02 02 00 dc 0a 01 03 30 23 02 01 0e 0a 01 01 30 1b 30 0e 30 0c 02 02 01 68 30 04 05 00 05 00 05 00 30 09 05 00 02 02 00 82 0a 01 03 30 5e 30 30 5b 30 08 02 01 00 30 03 02 01 00 30 08 02 01 01 30 03 02 01 00 30 08 02 01 02 30 03 02 01 00 30 08 02 01 03 30 03 02 01 00 30 08 02 01 04 30 03 02 01 00 30 08 02 01 05 30 03 02 01 00 30 08 02 01 06 30 03 02 01 00 30 13 02 01 08 30 0e 30 0c 30 30 03 02 01 0b 02 01 0f 02 01 00

- No.: 166
- Timestamp: 20:48:29:238_0
- RFN: 128
- Chip: 21760
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Config_CNF
- Source: ts_SS_PCH_FACH_CCCH_Cfg LINE 6
- Message Structure:
CPHY_TrCH_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 5
- Constraint:
ca_TrChCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 05

- No.: 167
- Timestamp: 20:48:29:278_0
- RFN: 132
- Chip: 20736
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_SS_PCH_FACH_CCCH_Cfg LINE 7
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 5
. (RatType)ratType = 0
. configMessage
. . CmacConfigReq
. . . SS_ActivationTime
. . . UE_Info
. . . . U_RNTI
. . . . (BitStringType)c_RNTI[16] = -
. . . TrCHInfo
. . . . ulconnectedTrCHList
. . . . TFCS
. . . . dlconnectedTrCHList
. . . . . TrCHInfo_setseq_1
. . . . . . (IntegerType)trchid = 12
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 240
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional = 0
. . . . . . . . (IntegerType)rateMatchingAttribute = 230
. . . . . . . . (CRC_Size)crc_Size = 3
. . . . . TrCHInfo_setseq_1
. . . . . . (IntegerType)trchid = 13
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 168
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . (IntegerType)small = 2
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional = 0
. . . . . . . . (IntegerType)rateMatchingAttribute = 220
. . . . . . . . (CRC_Size)crc_Size = 3
. . . . . TrCHInfo_setseq_1
. . . . . . (IntegerType)trchid = 14
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 360
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . (IntegerType)rateMatchingAttribute = 130
. . . . . . . . (CRC_Size)crc_Size = 3
. . . . TFCS
. . . . . ExplicitTFCS_Configuration
. . . . . . TFCS_ReconfAdd
. . . . . . . ctfcSize
. . . . . . . . ctfc4Bit
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 0
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 1
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 2
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 3
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 4
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 5
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 6
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 8
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 11
. . . . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . TrCH_LogCHMappingList1
. . . . ulconnectedTrCHList
. . . . dlconnectedTrCHList
. . . . . TrCH_LogCHMappingList1_setseq_1
. . . . . . (IntegerType)trchid = 12
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 3
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 1
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 1
. . . . . . . . (IntegerType)rB_Identity = -2
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . TrCH_LogCHMappingList1_setseq_1
. . . . . . (IntegerType)trchid = 13
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 1
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 5
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 2
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 1
. . . . . . . . (IntegerType)rB_Identity = 0
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_CMAC_CfgInfo
- BinaryMessage:
30 82 01 23 02 01 00 02 01 05 0a 01 00 30 82 01 16 05 00 30 00 30 81 cd 30 6b 30 21 02 01 0c 30 1c 30 0e 30 0c 02 02 00 f0 30 04 05 00 05 00 05 00 30 0a 0a 01 00 02 02 00 e6 0a 01 03 30 24 02 01 0d 30 1f 30 11 30 0f 02 02 00 a8 30 07 05 00 05 00 02 01 02 05 00 30 0a 0a 01 00 02 02 00 dc 0a 01 03 30 20 02 01 0e 30 1b 30 0e 30 0c 02 02 01 68 30 04 05 00 05 00 05 00 30 09 05 00 02 02 00 82 0a 01 03 30 5e 30 30 5b 30 08 02 01 00 30 03 02 01 00 30 08 02 01 01 30 03 02 01 00 30 08 02 01 02 30 03 02 01 00 30 08 02 01 03 30 03 02 01 00 30 08 02 01 04 30 03 02 01 00 30 08 02 01 05 30 03 02 01 00 30 08 02 01 06 30 03 02 01 00 30 13 02 01 08 30 0e 30 0c 30 30 03 02 01 0b 02 01 0f 02 01 00 30 40 30 3e 30 1d 02 01 0c 30 18 30 16 30 11 0a 01 00 0a 01 03 02 01 01 0a 01 01 05 00 02 01 01 02 01 fe 30 1d 02 01 0d 30 18 30 16 30 11 0a 01 00 0a 01 01 02 01 05 0a 01 02 05 00 02 01 01 02 01 00

- No.: 171
- Timestamp: 20:48:29:325_0
- RFN: 137
- Chip: 9728
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_SS_PCH_FACH_CCCH_Cfg LINE 8
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 5
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 05

- No.: 172
- Timestamp: 20:48:29:330_0
- RFN: 137
- Chip: 27136
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_PCH_FACH_CCCH_Cfg LINE 9
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 6
. (RatType)ratType = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . PICHInfo
. . . . PICH_Info
. . . . . fdd
. . . . . . (IntegerType)channelisationCode256 = 2
. . . . . . (PI_CountPerFrame)pi_CountPerFrame = 0
. . . . . . (BooleanType)sttd_Indicator = FALSE
. . . . (IntegerType)dl_TxPower = -5
- Constraint:
ca_PICH_Info
- BinaryMessage:
30 1c 02 01 00 02 01 06 0a 01 00 30 11 30 0f 30 30 09 02 01 02 0a 01 00 01 01 00 02 01 fb

- No.: 176
- Timestamp: 20:48:29:338_0
- RFN: 138
- Chip: 20224
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_PCH_FACH_CCCH_Cfg LINE 10
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 6
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 06

- No.: 184
- Timestamp: 20:48:29:344_0
- RFN: 139
- Chip: 3584
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_RACH_CCCH_Cfg LINE 3
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 7
. (RatType)ratType = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . AICHInfo
. . . . AICH_Info
. . . . . (IntegerType)channelisationCode256 = 3
. . . . . (BooleanType)sttd_Indicator = FALSE
. . . . . (AICH_TransmissionTiming)aich_TransmissionTiming = 0
. . . . (IntegerType)dl_TxPower = -5
- Constraint:
ca_AichInfo
- BinaryMessage:
30 1b 02 01 00 02 01 07 0a 01 00 30 10 30 0e 30 09 02 01 03 01 01 00 0a 01 00 02 01 fb

- No.: 188
- Timestamp: 20:48:29:351_0
- RFN: 139
- Chip: 34304
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_RACH_CCCH_Cfg LINE 4
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 7
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 07

- No.: 189
- Timestamp: 20:48:29:356_0
- RFN: 140
- Chip: 13568
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_RACH_CCCH_Cfg LINE 5
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 8
. (RatType)ratType = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . PRACHInfo
. . . . fdd_tdd
. . . . . fdd
. . . . . . (BitStringType)preambleSignature[16] = "0000000011111111"
. . . . . . (SF_PRACH)spreadingFactorForDataPart = 1
. . . . . . (IntegerType)preambleScramblingCode = 0
. . . . . . (PuncturingLimit)puncturingLimit = 15
. . . . . . (BitStringType)accessSlot[12] = "111111111111"
- Constraint:
ca_PRACH_Info
- BinaryMessage:
30 23 02 01 00 02 01 08 0a 01 00 30 18 30 16 30 30 13 03 03 00 00 ff 0a 01 01 02 01 00 0a 01 0f 03 03 04 ff f0

- No.: 193
- Timestamp: 20:48:29:365_0
- RFN: 141
- Chip: 9728
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_RACH_CCCH_Cfg LINE 6
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 8
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 08

- No.: 194
- Timestamp: 20:48:29:376_0
- RFN: 142
- Chip: 11776
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Config_REQ
- Source: ts_SS_RACH_CCCH_Cfg LINE 7
- Message Structure:
CPHY_TrCH_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 8
. (RatType)ratType = 0
. CphyTrchConfigReq
. . SS_ActivationTime
. . ulconnectedTrCHList
. . . CphyTrchConfigReq_setseq_0
. . . . (IntegerType)trchid = 15
. . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 1
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 168
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 360
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional = 0
. . . . . . (IntegerType)rateMatchingAttribute = 150
. . . . . . (CRC_Size)crc_Size = 3
. . TFCS
. . . ExplicitTFCS_Configuration
. . . . TFCS_ReconfAdd
. . . . . ctfcSize
. . . . . . ctfc2Bit
. . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . (IntegerType)ctfc2 = 0
. . . . . . . . PowerOffsetInformation
. . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . (IntegerType)ctfc2 = 1
. . . . . . . . PowerOffsetInformation
. . dlconnectedTrCHList
. . TFCS
- Constraint:
cab_RACH_InfoActNow
- BinaryMessage:
30 4e 02 01 00 02 01 08 0a 01 00 30 43 05 00 30 30 30 2e 02 01 0f 0a 01 01 30 26 30 18 30 0a 02 02 00 a8 30 02 05 00 05 00 30 0a 02 02 01 68 30 02 05 00 05 00 30 0a 0a 01 00 02 02 00 96 0a 01 03 30 0d 30 30 0a 30 03 02 01 00 30 03 02 01 01

- No.: 198
- Timestamp: 20:48:29:384_0
- RFN: 143
- Chip: 4352
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Config_CNF
- Source: ts_SS_RACH_CCCH_Cfg LINE 8
- Message Structure:
CPHY_TrCH_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 8
- Constraint:
ca_TrChCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 08

- No.: 199
- Timestamp: 20:48:29:401_0
- RFN: 144
- Chip: 33536
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_SS_RACH_CCCH_Cfg LINE 9
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 8
. (RatType)ratType = 0
. configMessage
. . CmacConfigReq
. . . SS_ActivationTime
. . . UE_Info
. . . . U_RNTI
. . . . (BitStringType)c_RNTI[16] = -
. . . TrCHInfo
. . . . ulconnectedTrCHList
. . . . . TrCHInfo_setseq_0
. . . . . . (IntegerType)trchid = 15
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 168
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 360
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional = 0
. . . . . . . . (IntegerType)rateMatchingAttribute = 150
. . . . . . . . (CRC_Size)crc_Size = 3
. . . . TFCS
. . . . . ExplicitTFCS_Configuration
. . . . . . TFCS_ReconfAdd
. . . . . . . ctfcSize
. . . . . . . . ctfc2Bit
. . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . (IntegerType)ctfc2 = 0
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . (IntegerType)ctfc2 = 1
. . . . . . . . . . PowerOffsetInformation
. . . . dlconnectedTrCHList
. . . . TFCS
. . . TrCH_LogCHMappingList1
. . . . ulconnectedTrCHList
. . . . . TrCH_LogCHMappingList1_setseq_0
. . . . . . (IntegerType)trchid = 15
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 1
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 5
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 2
. . . . . . . . (IntegerType)rB_Identity = 0
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . dlconnectedTrCHList
- Constraint:
ca_CMAC_CfgInfo
- BinaryMessage:
30 6d 02 01 00 02 01 08 0a 01 00 30 62 05 00 30 00 30 3e 30 2d 30 2b 02 01 0f 30 26 30 18 30 0a 02 02 00 a8 30 02 05 00 05 00 30 0a 02 02 01 68 30 02 05 00 05 00 30 0a 0a 01 00 02 02 00 96 0a 01 03 30 0d 30 30 0a 30 03 02 01 00 30 03 02 01 01 30 1c 30 1a 30 18 02 01 0f 30 13 30 11 30 0c 0a 01 00 0a 01 01 02 01 05 0a 01 02 02 01 00

- No.: 203
- Timestamp: 20:48:29:408_0
- RFN: 145
- Chip: 21504
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_SS_RACH_CCCH_Cfg LINE 10
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 8
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 08

- No.: 240
- Timestamp: 20:48:29:427_0
- RFN: 147
- Chip: 16640
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_1DCH_DCCH_Cfg LINE 4
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
. (RatType)ratType = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . DPCHInfo
. . . . UL_DPCH_Info
. . . . DL_DPCHInfo
. . . . . DL_CommonInformation
. . . . . . DL_DPCH_InfoCommon
. . . . . . . cfnHandling
. . . . . . . . initialise
. . . . . . . . . (IntegerType)cfntargetsfnframeoffset = -
. . . . . . . modeSpecificInfo
. . . . . . . . fdd
. . . . . . . . . DL_DPCH_PowerControlInfo
. . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . fdd
. . . . . . . . . . . . (DPC_Mode)dpc_Mode = 0
. . . . . . . . . (IntegerType)powerOffsetPilot_pdpdch = 0
. . . . . . . . . Dl_rate_matching_restriction
. . . . . . . . . SF512_AndPilot
. . . . . . . . . . (PilotBits128)sfd128 = 0
. . . . . . . . . (PositionFixedOrFlexible)positionFixedOrFlexible = 0
. . . . . . . . . (BooleanType)tfci_Existence = FALSE
. . . . . . modeSpecificInfo
. . . . . . . fdd
. . . . . . . . (IntegerType)defaultDPCH_OffsetValue = 0
. . . . . . . . DPCH_CompressedModeInfo
. . . . . . . . (TX_DiversityMode)tx_DiversityMode = 0
. . . . . . . . SSDT_Information
. . . . . DL_DPCH_InfoPerRL
. . . . . . fdd
. . . . . . . (PCPICH_UsageForChannelEst)pCPICH_UsageForChannelEst = 0
. . . . . . . (IntegerType)dpch_FrameOffset = 0
. . . . . . . SecondaryCPICH_Info
. . . . . . . DL_ChannelisationCodeList
. . . . . . . . DL_ChannelisationCode
. . . . . . . . . (IntegerType)secondaryScramblingCode = 1
. . . . . . . . . SF512_AndCodeNumber
. . . . . . . . . . (IntegerType)sf128 = 0
. . . . . . . . . (ScramblingCodeChange)scramblingCodeChange = -
. . . . . . . (IntegerType)tpc_CombinationIndex = 0
. . . . . . . (SSDT_CellIdentity)ssdt_CellIdentity = -
. . . . . . . (ClosedLoopTimingAdjMode)closedLoopTimingAdjMode = -
. . . . . (IntegerType)powerOffsetOfTFCI_PO1 = 0
. . . . . (IntegerType)powerOffsetOfTPC_PO2 = 0
. . . . . (IntegerType)powerOffsetOfPILOT_PO3 = 0
. . . . . (IntegerType)dl_TxPower = -5
. . . . . (IntegerType)dl_TxPowerMax = 15
. . . . . (IntegerType)dl_TxPowerMin = -35
- Constraint:
ca_DL_DPCH_Info
- BinaryMessage:
30 5e 02 01 00 02 01 1a 0a 01 00 30 53 30 51 30 4f 30 25 30 1a 30 30 00 30 30 14 30 06 30 30 03 0a 01 00 02 01 00 0a 01 00 0a 01 00 01 01 00 30 30 06 02 01 00 0a 01 00 30 30 13 0a 01 00 02 01 00 30 08 30 06 02 01 01 02 01 00 02 01 00 02 01 00 02 01 00 02 01 00 02 01 fb 02 01 0f 02 01 dd

- No.: 244
- Timestamp: 20:48:29:434_0
- RFN: 148
- Chip: 7936
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_1DCH_DCCH_Cfg LINE 5
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 1a

- No.: 245
- Timestamp: 20:48:29:447_0
- RFN: 149
- Chip: 17408
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Config_REQ
- Source: ts_SS_1DCH_DCCH_Cfg LINE 6
- Message Structure:
CPHY_TrCH_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
. (RatType)ratType = 0
. CphyTrchConfigReq
. . SS_ActivationTime
. . ulconnectedTrCHList
. . TFCS
. . dlconnectedTrCHList
. . . CphyTrchConfigReq_setseq_1
. . . . (IntegerType)trchid = 10
. . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 148
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional = 1
. . . . . . (IntegerType)rateMatchingAttribute = 192
. . . . . . (CRC_Size)crc_Size = 3
. . TFCS
. . . ExplicitTFCS_Configuration
. . . . TFCS_ReconfAdd
. . . . . ctfcSize
. . . . . . ctfc2Bit
. . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . (IntegerType)ctfc2 = 0
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . (IntegerType)ctfc2 = 1
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . fdd
. . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 11
. . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
- Constraint:
ca_DCH_148_TTI_10_DL_InfoActNow
- BinaryMessage:
30 59 02 01 00 02 01 1a 0a 01 00 30 4e 05 00 30 26 30 24 02 01 0a 0a 01 00 30 1c 30 0e 30 0c 02 02 00 94 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 c0 0a 01 03 30 22 30 30 1f 30 08 02 01 00 30 03 02 01 00 30 13 02 01 01 30 0e 30 0c 30 30 03 02 01 0b 02 01 0f 02 01 00

- No.: 249
- Timestamp: 20:48:29:455_0
- RFN: 150
- Chip: 8960
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Config_CNF
- Source: ts_SS_1DCH_DCCH_Cfg LINE 7
- Message Structure:
CPHY_TrCH_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
ca_TrChCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 1a

- No.: 250
- Timestamp: 20:48:29:489_0
- RFN: 153
- Chip: 22016
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_SS_1DCH_DCCH_Cfg LINE 8
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
. (RatType)ratType = 0
. configMessage
. . CmacConfigReq
. . . SS_ActivationTime
. . . UE_Info
. . . . U_RNTI
. . . . (BitStringType)c_RNTI[16] = -
. . . TrCHInfo
. . . . ulconnectedTrCHList
. . . . TFCS
. . . . dlconnectedTrCHList
. . . . . TrCHInfo_setseq_1
. . . . . . (IntegerType)trchid = 10
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 148
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . (IntegerType)rateMatchingAttribute = 192
. . . . . . . . (CRC_Size)crc_Size = 3
. . . . TFCS
. . . . . ExplicitTFCS_Configuration
. . . . . . TFCS_ReconfAdd
. . . . . . . ctfcSize
. . . . . . . . ctfc2Bit
. . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . (IntegerType)ctfc2 = 0
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . (IntegerType)ctfc2 = 1
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 11
. . . . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . TrCH_LogCHMappingList1
. . . . ulconnectedTrCHList
. . . . dlconnectedTrCHList
. . . . . TrCH_LogCHMappingList1_setseq_1
. . . . . . (IntegerType)trchid = 10
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 1
. . . . . . . . (IntegerType)rB_Identity = 1
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 2
. . . . . . . . (IntegerType)rB_Identity = 2
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 3
. . . . . . . . (IntegerType)rB_Identity = 3
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 4
. . . . . . . . (IntegerType)rB_Identity = 4
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_CMAC_CfgInfo
- BinaryMessage:
30 81 c6 02 01 ff 02 01 1a 0a 01 00 30 81 ba 05 00 30 00 30 49 30 23 30 21 02 01 0a 30 1c 30 0e 30 0c 02 02 00 94 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 c0 0a 01 03 30 22 30 30 1f 30 08 02 01 00 30 03 02 01 00 30 13 02 01 01 30 0e 30 0c 30 30 03 02 01 0b 02 01 0f 02 01 00 30 69 30 67 30 65 02 01 0a 30 60 30 16 30 11 0a 01 00 0a 01 00 02 01 01 0a 01 04 05 00 02 01 01 02 01 01 30 16 30 11 0a 01 00 0a 01 00 02 01 02 0a 01 04 05 00 02 01 02 02 01 02 30 16 30 11 0a 01 00 0a 01 00 02 01 03 0a 01 04 05 00 02 01 03 02 01 03 30 16 30 11 0a 01 00 0a 01 00 02 01 04 0a 01 04 05 00 02 01 04 02 01 04

- No.: 254
- Timestamp: 20:48:29:512_0
- RFN: 155
- Chip: 33024
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_SS_1DCH_DCCH_Cfg LINE 9
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 1a

- No.: 255
- Timestamp: 20:48:29:518_0
- RFN: 156
- Chip: 18176
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_1DCH_DCCH_Cfg LINE 10
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
. (RatType)ratType = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . DPCHInfo
. . . . UL_DPCH_Info
. . . . . UL_DPCH_PowerControlInfo
. . . . . . fdd
. . . . . . . (IntegerType)dpcch_PowerOffset = -40
. . . . . . . (IntegerType)pc_Preamble = 1
. . . . . . . (IntegerType)sRB_delay = 7
. . . . . . . PowerControlAlgorithm
. . . . . . . . (IntegerType)algorithm1 = 1
. . . . . modeSpecificInfo
. . . . . . fdd
. . . . . . . (ScramblingCodeType)scramblingCodeType = 1
. . . . . . . (IntegerType)scramblingCode = 0
. . . . . . . (IntegerType)numberOfDPDCH = -
. . . . . . . (SpreadingFactor)spreadingFactor = 4
. . . . . . . (BooleanType)tfci_Existence = TRUE
. . . . . . . (IntegerType)numberOfFBI_Bits = -
. . . . . . . (PuncturingLimit)puncturingLimit = 15
. . . . DL_DPCHInfo
- Constraint:
ca_UL_DPCH_Info
- BinaryMessage:
30 30 02 01 00 02 01 14 0a 01 00 30 25 30 23 30 21 30 30 0c 02 01 d8 02 01 01 02 01 07 02 01 01 30 30 0f 0a 01 01 02 01 00 0a 01 04 01 01 ff 0a 01 0f

- No.: 259
- Timestamp: 20:48:29:524_0
- RFN: 157
- Chip: 5120
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_1DCH_DCCH_Cfg LINE 11
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 260
- Timestamp: 20:48:29:534_0
- RFN: 158
- Chip: 2816
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Config_REQ
- Source: ts_SS_1DCH_DCCH_Cfg LINE 12
- Message Structure:
CPHY_TrCH_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
. (RatType)ratType = 0
. CphyTrchConfigReq
. . SS_ActivationTime
. . ulconnectedTrCHList
. . . CphyTrchConfigReq_setseq_0
. . . . (IntegerType)trchid = 5
. . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 148
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional = 1
. . . . . . (IntegerType)rateMatchingAttribute = 192
. . . . . . (CRC_Size)crc_Size = 3
. . TFCS
. . . ExplicitTFCS_Configuration
. . . . TFCS_ReconfAdd
. . . . . ctfcSize
. . . . . . ctfc2Bit
. . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . (IntegerType)ctfc2 = 0
. . . . . . . . PowerOffsetInformation
. . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . (IntegerType)ctfc2 = 1
. . . . . . . . PowerOffsetInformation
. . dlconnectedTrCHList
. . TFCS
- Constraint:
ca_DCH_148_TTI_10_UL_InfoActNow
- BinaryMessage:
30 44 02 01 00 02 01 14 0a 01 00 30 39 05 00 30 26 30 24 02 01 05 0a 01 00 30 1c 30 0e 30 0c 02 02 00 94 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 c0 0a 01 03 30 0d 30 30 0a 30 03 02 01 00 30 03 02 01 01

- No.: 264
- Timestamp: 20:48:29:544_0
- RFN: 159
- Chip: 5376
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Config_CNF
- Source: ts_SS_1DCH_DCCH_Cfg LINE 13
- Message Structure:
CPHY_TrCH_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_TrChCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 265
- Timestamp: 20:48:29:576_0
- RFN: 162
- Chip: 13824
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_SS_1DCH_DCCH_Cfg LINE 14
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
. (RatType)ratType = 0
. configMessage
. . CmacConfigReq
. . . SS_ActivationTime
. . . UE_Info
. . . . U_RNTI
. . . . (BitStringType)c_RNTI[16] = -
. . . TrCHInfo
. . . . ulconnectedTrCHList
. . . . . TrCHInfo_setseq_0
. . . . . . (IntegerType)trchid = 5
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 148
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . (IntegerType)rateMatchingAttribute = 192
. . . . . . . . (CRC_Size)crc_Size = 3
. . . . TFCS
. . . . . ExplicitTFCS_Configuration
. . . . . . TFCS_ReconfAdd
. . . . . . . ctfcSize
. . . . . . . . ctfc2Bit
. . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . (IntegerType)ctfc2 = 0
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . (IntegerType)ctfc2 = 1
. . . . . . . . . . PowerOffsetInformation
. . . . dlconnectedTrCHList
. . . . TFCS
. . . TrCH_LogCHMappingList1
. . . . ulconnectedTrCHList
. . . . . TrCH_LogCHMappingList1_setseq_0
. . . . . . (IntegerType)trchid = 5
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . (IntegerType)rB_Identity = 1
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . (IntegerType)rB_Identity = 2
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . (IntegerType)rB_Identity = 3
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . (IntegerType)rB_Identity = 4
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . dlconnectedTrCHList
- Constraint:
ca_CMAC_CfgInfo
- BinaryMessage:
30 81 9d 02 01 ff 02 01 14 0a 01 00 30 81 91 05 00 30 00 30 34 30 23 30 21 02 01 05 30 1c 30 0e 30 0c 02 02 00 94 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 c0 0a 01 03 30 0d 30 30 0a 30 03 02 01 00 30 03 02 01 01 30 55 30 53 30 51 02 01 05 30 4c 30 11 30 0c 0a 01 00 0a 01 00 02 01 01 0a 01 04 02 01 01 30 11 30 0c 0a 01 00 0a 01 00 02 01 02 0a 01 04 02 01 02 30 11 30 0c 0a 01 00 0a 01 00 02 01 03 0a 01 04 02 01 03 30 11 30 0c 0a 01 00 0a 01 00 02 01 04 0a 01 04 02 01 04

- No.: 269
- Timestamp: 20:48:29:599_0
- RFN: 164
- Chip: 22528
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_SS_1DCH_DCCH_Cfg LINE 15
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 14

- No.: 272
- Timestamp: 20:48:29:605_0
- RFN: 165
- Chip: 6912
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB_BCCH_BCH_Cfg LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 246
. . . . . UL_RLC_Mode
. . . . . . UL_TM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . (BooleanType)segmentationIndication = FALSE
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = -
. . . . (IntegerType)dLlogicalChannelIdentity = 1
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_BCCH_Info
- BinaryMessage:
30 1d 02 01 00 02 01 ff 0a 01 00 30 12 30 0b 30 09 02 02 00 f6 30 03 01 01 00 30 03 02 01 01

- No.: 276
- Timestamp: 20:48:29:612_0
- RFN: 165
- Chip: 34048
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB_BCCH_BCH_Cfg LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 279
- Timestamp: 20:48:29:617_0
- RFN: 166
- Chip: 17408
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB_PCCH_Cfg LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -2
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 240
. . . . . UL_RLC_Mode
. . . . . . UL_TM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . (BooleanType)segmentationIndication = FALSE
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = -
. . . . (IntegerType)dLlogicalChannelIdentity = 1
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_PCCH_Info
- BinaryMessage:
30 1d 02 01 00 02 01 fe 0a 01 00 30 12 30 0b 30 09 02 02 00 f0 30 03 01 01 00 30 03 02 01 01

- No.: 283
- Timestamp: 20:48:29:622_0
- RFN: 166
- Chip: 36352
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB_PCCH_Cfg LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 fe

- No.: 286
- Timestamp: 20:48:29:628_0
- RFN: 167
- Chip: 20480
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB0_Cfg LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 152
. . . . . UL_RLC_Mode
. . . . . . UL_UM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (NoExplicitDiscard)timerBasedNoExplicit = 9
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = -
. . . . (IntegerType)dLlogicalChannelIdentity = 5
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_UM_DL_Info
- BinaryMessage:
30 1d 02 01 00 02 01 00 0a 01 00 30 12 30 0b 30 09 02 02 00 98 30 03 0a 01 09 30 03 02 01 05

- No.: 290
- Timestamp: 20:48:29:635_0
- RFN: 168
- Chip: 9984
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB0_Cfg LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 00

- No.: 291
- Timestamp: 20:48:29:641_0
- RFN: 168
- Chip: 33792
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB0_Cfg LINE 3
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_TM_RLC_Mode
. . . . . . (BooleanType)segmentationIndication = TRUE
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 166
. . . . . UL_RLC_Mode
. . . . . . UL_TM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . (BooleanType)segmentationIndication = TRUE
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = 5
. . . . (IntegerType)dLlogicalChannelIdentity = -
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_TM_UL_Info
- BinaryMessage:
30 22 02 01 00 02 01 00 0a 01 00 30 17 30 10 30 03 01 01 ff 30 09 02 02 00 a6 30 03 01 01 ff 30 03 02 01 05

- No.: 295
- Timestamp: 20:48:29:651_0
- RFN: 169
- Chip: 31488
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB0_Cfg LINE 4
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 00

- No.: 298
- Timestamp: 20:48:29:658_0
- RFN: 170
- Chip: 20480
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 136
. . . . . UL_RLC_Mode
. . . . . . UL_UM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (NoExplicitDiscard)timerBasedNoExplicit = 9
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = 1
. . . . (IntegerType)dLlogicalChannelIdentity = 1
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_UM_Info
- BinaryMessage:
30 22 02 01 ff 02 01 01 0a 01 00 30 17 30 0d 05 00 30 09 02 02 00 88 30 03 0a 01 09 30 06 02 01 01 02 01 01

- No.: 302
- Timestamp: 20:48:29:670_0
- RFN: 171
- Chip: 27392
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 303
- Timestamp: 20:48:29:678_0
- RFN: 172
- Chip: 22016
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 3
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . (TimerEPC)timerEPC = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . (TimerRST)timerRST = 9
. . . . . . . (MaxRST)max_RST = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = 2
. . . . (IntegerType)dLlogicalChannelIdentity = 2
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 02 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 27 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 02 02 01 02

- No.: 307
- Timestamp: 20:48:29:700_0
- RFN: 174
- Chip: 28416
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 4
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 308
- Timestamp: 20:48:29:709_0
- RFN: 175
- Chip: 24320
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 5
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . (TimerEPC)timerEPC = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . (TimerRST)timerRST = 9
. . . . . . . (MaxRST)max_RST = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = 3
. . . . (IntegerType)dLlogicalChannelIdentity = 3
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 03 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 27 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 03 02 01 03

- No.: 312
- Timestamp: 20:48:29:731_0
- RFN: 177
- Chip: 32000
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 6
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 313
- Timestamp: 20:48:29:740_0
- RFN: 178
- Chip: 28160
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 7
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . (TimerEPC)timerEPC = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . (TimerRST)timerRST = 9
. . . . . . . (MaxRST)max_RST = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = 4
. . . . (IntegerType)dLlogicalChannelIdentity = 4
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 04 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 27 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 04 02 01 04

- No.: 317
- Timestamp: 20:48:29:761_0
- RFN: 180
- Chip: 31744
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 8
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 358
- Timestamp: 20:48:29:807_0
- RFN: 185
- Chip: 13312
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 27
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 1b

- No.: 363
- Timestamp: 20:48:29:812_0
- RFN: 185
- Chip: 33792
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendNoSegDefSchedul LINE 2
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 364
- Timestamp: 20:48:29:816_0
- RFN: 186
- Chip: 11264
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendNoSegDefSchedul LINE 3
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 08 02 01 00 02 01 ff 00 00

- No.: 372
- Timestamp: 20:48:29:826_0
- RFN: 187
- Chip: 11776
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 11
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 0b

- No.: 377
- Timestamp: 20:48:29:833_0
- RFN: 188
- Chip: 512
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB1 LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 378
- Timestamp: 20:48:29:839_0
- RFN: 188
- Chip: 21504
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB1 LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 1
. . . . . . . (BitStringType)sib_Data_variable[-1] = "1100010000000000000001011000100000101000000010100001000111100000000101000000000000000000000011000111010000"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 2
. . . . . . . (BitStringType)sib_Data_variable[-1] = "10000000000000000001"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 1c 02 01 00 02 01 ff 00 0e 21 69 c4 00 05 88 28 0a 11 e0 14 00 00 0c 74 04 27 00 00 20

- No.: 391
- Timestamp: 20:48:29:849_0
- RFN: 189
- Chip: 21504
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 11
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 0b

- No.: 396
- Timestamp: 20:48:29:853_0
- RFN: 190
- Chip: 768
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB2 LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 397
- Timestamp: 20:48:29:858_0
- RFN: 190
- Chip: 19456
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB2 LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 1
. . . . . . . (BitStringType)sib_Data_variable[-1] = "1100010000000000000001011000100000101000000010100001000111100000000101000000000000000000000011000111010000"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 2
. . . . . . . (BitStringType)sib_Data_variable[-1] = "10000000000000000001"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 1c 02 01 00 02 01 ff 00 0e 21 69 c4 00 05 88 28 0a 11 e0 14 00 00 0c 74 04 27 00 00 20

- No.: 409
- Timestamp: 20:48:29:868_0
- RFN: 191
- Chip: 19712
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 10
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 0a

- No.: 414
- Timestamp: 20:48:29:873_0
- RFN: 192
- Chip: 512
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB3 LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 415
- Timestamp: 20:48:29:878_0
- RFN: 192
- Chip: 20224
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB3 LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 7
. . . . . . . (BitStringType)sib_Data_variable[-1] = "101000101000000010000001"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 3
. . . . . . . (BitStringType)sib_Data_variable[-1] = "110000000000000000000000000000000100000011001100011000000000100100001000000100011111111111111111111111"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 1c 02 01 00 02 01 ff 00 0e 27 17 a2 80 81 1b 2e 00 00 00 02 06 63 00 48 40 8f ff ff e0

- No.: 427
- Timestamp: 20:48:29:888_0
- RFN: 193
- Chip: 19456
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 26
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 1a

- No.: 432
- Timestamp: 20:48:29:893_0
- RFN: 194
- Chip: 256
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB4 LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 433
- Timestamp: 20:48:29:898_0
- RFN: 194
- Chip: 19968
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB4 LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 7
. . . . . . . (BitStringType)sib_Data_variable[-1] = "101000101000000010000001"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 4
. . . . . . . (BitStringType)sib_Data_variable[-1] = "1000000000000000000000000000000101100110001100000000010010000100000010001110111"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 19 02 01 00 02 01 ff 00 0e 27 17 a2 80 81 22 74 00 00 00 0b 31 80 24 20 47 70

- No.: 450
- Timestamp: 20:48:29:946_0
- RFN: 199
- Chip: 11776
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 23
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 17

- No.: 455
- Timestamp: 20:48:29:952_0
- RFN: 199
- Chip: 34048
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB5 LINE 41
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 456
- Timestamp: 20:48:29:955_0
- RFN: 200
- Chip: 9216
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB5 LINE 42
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 08 02 01 00 02 01 ff 00 00

- No.: 460
- Timestamp: 20:48:29:959_0
- RFN: 200
- Chip: 25088
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 19
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 13

- No.: 465
- Timestamp: 20:48:29:972_0
- RFN: 201
- Chip: 34816
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB5 LINE 44
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 466
- Timestamp: 20:48:29:976_0
- RFN: 202
- Chip: 14848
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB5 LINE 45
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . FirstSegment
. . . . . . (SIB_Type)sib_Type = 5
. . . . . . (IntegerType)seg_Count = 3
. . . . . . (BitStringType)sib_Data_fixed[222] = "001101010100010000111110000000001111111101000011111111111111110111010010000100001111000000101001000011000000101010100101010110000000000000001100110001011011010101111110001010111010000011111110100000111111101000001111111010"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 25 02 01 00 02 01 ff 00 02 52 35 44 3e 00 ff 43 ff fd d2 10 f0 29 0c 0a a5 58 00 0c c5 b5 7e 2b a0 fe 83 fa 0f e8

- No.: 470
- Timestamp: 20:48:29:981_0
- RFN: 202
- Chip: 32256
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 21
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 15

- No.: 475
- Timestamp: 20:48:29:992_0
- RFN: 203
- Chip: 35584
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB5 LINE 47
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 476
- Timestamp: 20:48:29:996_0
- RFN: 204
- Chip: 15104
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB5 LINE 48
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . SubsequentSegment
. . . . . . (SIB_Type)sib_Type = 5
. . . . . . (IntegerType)segmentIndex = 1
. . . . . . (BitStringType)sib_Data_fixed[222] = "000011111111010000000000000000001101011000110100010000111111010011100101000001100001000011001010000000110000001110001001000000010110000000000000100000001110000000001000100001100100001010011001000010100000000000110000000100"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 25 02 01 00 02 01 ff 00 04 50 0f f4 00 00 d6 34 43 f4 e5 06 10 ca 03 03 89 01 60 00 80 e0 08 86 42 99 0a 00 30 10

- No.: 480
- Timestamp: 20:48:30:001_0
- RFN: 204
- Chip: 32768
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 22
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 16

- No.: 485
- Timestamp: 20:48:30:011_0
- RFN: 205
- Chip: 34560
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB5 LINE 50
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 487
- Timestamp: 20:48:30:016_0
- RFN: 206
- Chip: 14080
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB5 LINE 52
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . LastSegmentShort
. . . . . . (SIB_Type)sib_Type = 5
. . . . . . (IntegerType)segmentIndex = 2
. . . . . . (BitStringType)sib_Data_variable[-1] = "010001011100101011010110100000000000011110001000011000000001011011011011011000100000000001000011000010001001010000001011011010000000010000"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 1c 02 01 00 02 01 ff 00 06 51 89 45 ca d6 80 07 88 60 16 db 62 00 43 08 94 0b 68 04 00

- No.: 504
- Timestamp: 20:48:30:027_0
- RFN: 207
- Chip: 18944
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 3
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 03

- No.: 509
- Timestamp: 20:48:30:032_0
- RFN: 208
- Chip: 0
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB6 LINE 8
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 512
- Timestamp: 20:48:30:037_0
- RFN: 208
- Chip: 19456
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB6:lt_CompleteSIB LINE 4
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 6
. . . . . . . (BitStringType)sib_Data_variable[-1] = "0000001010010001"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 0c 02 01 00 02 01 ff 00 0e 06 0f 02 91

- No.: 517
- Timestamp: 20:48:30:042_0
- RFN: 208
- Chip: 36608
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 5
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 05

- No.: 522
- Timestamp: 20:48:30:051_0
- RFN: 209
- Chip: 35072
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB6 LINE 11
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 523
- Timestamp: 20:48:30:055_0
- RFN: 210
- Chip: 11520
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB6 LINE 12
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 08 02 01 00 02 01 ff 00 00

- No.: 527
- Timestamp: 20:48:30:059_0
- RFN: 210
- Chip: 26112
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 6
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 06

- No.: 532
- Timestamp: 20:48:30:071_0
- RFN: 211
- Chip: 34816
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB6 LINE 14
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 533
- Timestamp: 20:48:30:075_0
- RFN: 212
- Chip: 10240
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB6 LINE 15
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 08 02 01 00 02 01 ff 00 00

- No.: 537
- Timestamp: 20:48:30:079_0
- RFN: 212
- Chip: 25600
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 7
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 07

- No.: 542
- Timestamp: 20:48:30:091_0
- RFN: 213
- Chip: 35072
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB6 LINE 17
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 543
- Timestamp: 20:48:30:096_0
- RFN: 214
- Chip: 11520
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB6 LINE 18
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 08 02 01 00 02 01 ff 00 00

- No.: 551
- Timestamp: 20:48:30:110_0
- RFN: 215
- Chip: 25856
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 2
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 02

- No.: 556
- Timestamp: 20:48:30:117_0
- RFN: 216
- Chip: 16640
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB7 LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 559
- Timestamp: 20:48:30:125_0
- RFN: 217
- Chip: 8448
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB7:lt_CompleteSIB LINE 4
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 7
. . . . . . . (BitStringType)sib_Data_variable[-1] = "101000101000000010000001"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 0d 02 01 00 02 01 ff 00 0e 07 17 a2 80 81

- No.: 567
- Timestamp: 20:48:30:141_0
- RFN: 218
- Chip: 28672
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 10
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 0a

- No.: 572
- Timestamp: 20:48:30:148_0
- RFN: 219
- Chip: 18176
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB7:lt_ConcatWithSIB3 LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 573
- Timestamp: 20:48:30:154_0
- RFN: 220
- Chip: 4608
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB7:lt_ConcatWithSIB3 LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 7
. . . . . . . (BitStringType)sib_Data_variable[-1] = "101000101000000010000001"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 3
. . . . . . . (BitStringType)sib_Data_variable[-1] = "110000000000000000000000000000000100000011001100011000000000100100001000000100011111111111111111111111"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 1c 02 01 00 02 01 ff 00 0e 27 17 a2 80 81 1b 2e 00 00 00 02 06 63 00 48 40 8f ff ff e0

- No.: 581
- Timestamp: 20:48:30:168_0
- RFN: 221
- Chip: 20736
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 18
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 12

- No.: 586
- Timestamp: 20:48:30:176_0
- RFN: 222
- Chip: 10240
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB7:lt_ConcatWithSIB18 LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 587
- Timestamp: 20:48:30:182_0
- RFN: 222
- Chip: 35072
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB7:lt_ConcatWithSIB18 LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 7
. . . . . . . (BitStringType)sib_Data_variable[-1] = "101000101000000010000001"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 26
. . . . . . . (BitStringType)sib_Data_variable[-1] = "100100000001000000000001000000001"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 13 02 01 00 02 01 ff 00 0e 27 17 a2 80 81 d1 04 80 80 08 04

- No.: 595
- Timestamp: 20:48:30:196_0
- RFN: 224
- Chip: 11008
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 26
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 1a

- No.: 600
- Timestamp: 20:48:30:203_0
- RFN: 225
- Chip: 1024
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB7:lt_ConcatWithSIB4 LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 601
- Timestamp: 20:48:30:209_0
- RFN: 225
- Chip: 25344
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB7:lt_ConcatWithSIB4 LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 7
. . . . . . . (BitStringType)sib_Data_variable[-1] = "101000101000000010000001"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 4
. . . . . . . (BitStringType)sib_Data_variable[-1] = "1000000000000000000000000000000101100110001100000000010010000100000010001110111"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 19 02 01 00 02 01 ff 00 0e 27 17 a2 80 81 22 74 00 00 00 0b 31 80 24 20 47 70

- No.: 615
- Timestamp: 20:48:30:221_0
- RFN: 226
- Chip: 29696
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 31
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 1f

- No.: 620
- Timestamp: 20:48:30:225_0
- RFN: 227
- Chip: 9216
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB11 LINE 20
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 621
- Timestamp: 20:48:30:229_0
- RFN: 227
- Chip: 23040
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB11 LINE 21
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 08 02 01 00 02 01 ff 00 00

- No.: 625
- Timestamp: 20:48:30:233_0
- RFN: 228
- Chip: 512
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 29
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 1d

- No.: 630
- Timestamp: 20:48:30:243_0
- RFN: 228
- Chip: 37632
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB11 LINE 23
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 631
- Timestamp: 20:48:30:247_0
- RFN: 229
- Chip: 17152
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB11 LINE 24
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . FirstSegment
. . . . . . (SIB_Type)sib_Type = 11
. . . . . . (IntegerType)seg_Count = 2
. . . . . . (BitStringType)sib_Data_fixed[222] = "011000001101100100010010000000001000110010000100001000010010010110101000100000100110010001010011000001011001000010100111000010111000010100001000100010001100100101010100000001001010000101001010100001100001001010001000001010"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 25 02 01 00 02 01 ff 00 02 b1 60 d9 12 00 8c 84 21 25 a8 82 64 53 05 90 a7 0b 85 08 88 c9 54 04 a1 4a 86 12 88 28

- No.: 635
- Timestamp: 20:48:30:252_0
- RFN: 229
- Chip: 34560
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 30
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 1e

- No.: 640
- Timestamp: 20:48:30:261_0
- RFN: 230
- Chip: 33280
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB11 LINE 26
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 642
- Timestamp: 20:48:30:266_0
- RFN: 231
- Chip: 14080
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB11 LINE 28
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . LastSegmentShort
. . . . . . (SIB_Type)sib_Type = 11
. . . . . . (IntegerType)segmentIndex = 1
. . . . . . (BitStringType)sib_Data_variable[-1] = "000100001100001001010010011010101000011000010010101000101100011001010100101010100001001111101000100010000001010010110000100010100001010101111000"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 1c 02 01 00 02 01 ff 00 06 b0 8f 10 c2 52 6a 86 12 a2 c6 54 aa 13 e8 88 14 b0 8a 15 78

- No.: 655
- Timestamp: 20:48:30:276_0
- RFN: 232
- Chip: 11520
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 13
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 0d

- No.: 660
- Timestamp: 20:48:30:282_0
- RFN: 232
- Chip: 37632
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB12 LINE 8
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 663
- Timestamp: 20:48:30:287_0
- RFN: 233
- Chip: 18432
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB12:lt_CompleteSIB LINE 4
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 12
. . . . . . . (BitStringType)sib_Data_variable[-1] = "010000000"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 0c 02 01 00 02 01 ff 00 0e 0c 08 40 00

- No.: 668
- Timestamp: 20:48:30:292_0
- RFN: 233
- Chip: 35840
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 14
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 0e

- No.: 673
- Timestamp: 20:48:30:301_0
- RFN: 234
- Chip: 33280
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB12 LINE 11
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 674
- Timestamp: 20:48:30:305_0
- RFN: 235
- Chip: 10496
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB12 LINE 12
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 08 02 01 00 02 01 ff 00 00

- No.: 678
- Timestamp: 20:48:30:309_0
- RFN: 235
- Chip: 26368
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 15
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 0f

- No.: 683
- Timestamp: 20:48:30:321_0
- RFN: 236
- Chip: 32768
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB12 LINE 14
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 684
- Timestamp: 20:48:30:325_0
- RFN: 237
- Chip: 9728
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB12 LINE 15
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 08 02 01 00 02 01 ff 00 00

- No.: 692
- Timestamp: 20:48:30:333_0
- RFN: 238
- Chip: 2560
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 6
. . (IntegerType)sg_POS = 18
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 12

- No.: 697
- Timestamp: 20:48:30:342_0
- RFN: 238
- Chip: 37632
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB18 LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 698
- Timestamp: 20:48:30:347_0
- RFN: 239
- Chip: 17408
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB18 LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 7
. . . . . . . (BitStringType)sib_Data_variable[-1] = "101000101000000010000001"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 26
. . . . . . . (BitStringType)sib_Data_variable[-1] = "100100000001000000000001000000001"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 13 02 01 00 02 01 ff 00 0e 27 17 a2 80 81 d1 04 80 80 08 04

- No.: 710
- Timestamp: 20:48:30:356_0
- RFN: 240
- Chip: 13056
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 4
. . (IntegerType)sg_POS = 1
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 04 02 01 01

- No.: 715
- Timestamp: 20:48:30:362_0
- RFN: 240
- Chip: 37888
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSB1_DefSchedul LINE 4
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 718
- Timestamp: 20:48:30:368_0
- RFN: 241
- Chip: 20224
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSB1_DefSchedul:lt_CompleteSIB LINE 4
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 27
. . . . . . . (BitStringType)sib_Data_variable[-1] = "10010000101010001000001100110000010010010100111000101001110100000000010110100010001101110010100010010010"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 17 02 01 00 02 01 ff 00 0e 1b 67 90 a8 83 30 49 4e 29 d0 05 a2 37 28 92

- No.: 736
- Timestamp: 20:48:30:379_0
- RFN: 242
- Chip: 25088
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP = 3
. . (IntegerType)sg_POS = 0
. . (IntegerType)bcch_ModificationTime = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 03 02 01 00

- No.: 741
- Timestamp: 20:48:30:383_0
- RFN: 243
- Chip: 4352
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendMIB LINE 7
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 744
- Timestamp: 20:48:30:389_0
- RFN: 243
- Chip: 25344
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendMIB:lt_CompleteSIB LINE 4
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type = 0
. . . . . . . (BitStringType)sib_Data_variable[-1] = "0001000000000000010000000010010110101010000100010000000000001000100010110000101000100010110001001000100010100001101000100110100010001110010010010011000100010000"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 1e 02 01 00 02 01 ff 00 0e 00 9f 10 00 40 25 aa 11 00 08 8b 0a 22 c4 88 a1 a2 68 8e 49 31 10

- No.: 759
- Timestamp: 20:48:30:395_0
- RFN: 244
- Chip: 12032
- Event: Send
- PCO: Ut
- Message: MMI_CmdReq
- Source: ts_MMI_UE_SwitchOn LINE 1
- Message Structure:
MMI_CmdReq
. (IA5StringType)cmd[-1] = "Please switch on the UE"
- Constraint:
ca_MMI_CmdReq
- BinaryMessage:
50 6c 65 61 73 65 20 73 77 69 74 63 68 20 6f 6e 20 74 68 65 20 55 45

- No.: 766
- Timestamp: 20:48:38:716_0
- RFN: 1076
- Chip: 13824
- Event: Receive
- PCO: Ut
- Message: MMI_CmdCnf
- Source: ts_MMI_UE_SwitchOn LINE 2
- Message Structure:
MMI_CmdCnf
. (BooleanType)result = TRUE
. (IA5StringType)resultString[6] = " OK "
- Constraint:
ca_MMI_CmdCnf
- BinaryMessage:
80 0d 0a 4f 4b 0d 0a

- No.: 782
- Timestamp: 20:48:38:727_0
- RFN: 1077
- Chip: 15104
- Event: Receive
- PCO: TM
- Message: RLC_TR_DATA_IND
- Source: ts_RRC_ConnEst:lt_RcvConnReq LINE 2
- Message Structure:
RLC_TR_DATA_IND
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
. tM_message
. . UL_CCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode = 0
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . UL_CCCH_MessageType
. . . . RRCConnectionRequest
. . . . . InitialUE_Identity
. . . . . . TMSI_and_LAI_GSM_MAP
. . . . . . . (BitStringType)tmsi[32] = "00010010001101000101011001111000"
. . . . . . . LAI
. . . . . . . . PLMN_Identity
. . . . . . . . . MCC
. . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . (IntegerType)_elem = 1
. . . . . . . . . MNC
. . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . (IntegerType)_elem = 1
. . . . . . . . (BitStringType)lac[16] = '0000000000000001'B
. . . . . (EstablishmentCause)establishmentCause = 12
. . . . . (ProtocolErrorIndicator)protocolErrorIndicator = 0
. . . . . MeasuredResultsOnRACH
. . . . . . currentCell
. . . . . . . modeSpecificInfo
. . . . . . . . fdd
. . . . . . . . . measurementQuantity
. . . . . . . . . . (IntegerType)cpich_Ec_N0 = 0
. . . . . v3d0NonCriticalExtensions
. . . . . . RRCConnectionRequest_v3d0ext_IEs
. . . . . . . (BitStringType)uESpecificBehaviourInformation1idle = 0
. . . . . . nonCriticalExtensions
- Constraint:
car_RRC_ConnReq
- BinaryMessage:
30 11 02 01 00 02 01 00 21 12 34 56 78 00 10 08 00 0b 00

- No.: 786
- Timestamp: 20:48:38:787_0
- RFN: 1083
- Chip: 17408
- Event: Send
- PCO: UM
- Message: RLC_UM_DATA_REQ
- Source: ts_RRC_ConnEst:lt_Send_ConnSetUp LINE 22
- Message Structure:
RLC_UM_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
. uM_message
. . DL_CCCH_Message
. . . IntegrityCheckInfo
. . . DL_CCCH_MessageType
. . . . RRCConnectionSetup
. . . . . r3
. . . . . . RRCConnectionSetup_r3_IEs
. . . . . . . InitialUE_Identity
. . . . . . . . TMSI_and_LAI_GSM_MAP
. . . . . . . . . (BitStringType)tmsi[32] = "00010010001101000101011001111000"
. . . . . . . . . LAI
. . . . . . . . . . PLMN_Identity
. . . . . . . . . . . MCC
. . . . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . . . (IntegerType)_elem = 1
. . . . . . . . . . . MNC
. . . . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . . . (IntegerType)_elem = 1
. . . . . . . . . . (BitStringType)lac[16] = '0000000000000001'B
. . . . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . . . (IntegerType)activationTime = -
. . . . . . . U_RNTI
. . . . . . . . (BitStringType)srnc_Identity[12] = "000000000001"
. . . . . . . . (BitStringType)s_RNTI[20] = "00000000000000000001"
. . . . . . . (BitStringType)new_c_RNTI[16] = -
. . . . . . . (RRC_StateIndicator)rrc_StateIndicator = 0
. . . . . . . (IntegerType)utran_DRX_CycleLengthCoeff = 9
. . . . . . . CapabilityUpdateRequirement
. . . . . . . . (BooleanType)ue_RadioCapabilityFDDUpdateRequirement = TRUE
. . . . . . . . (BooleanType)ue_RadioCapabilityTDDUpdateRequirement = FALSE
. . . . . . . . SystemSpecificCapUpdateReqList
. . . . . . . . . (SystemSpecificCapUpdateReq)_elem = 0
. . . . . . . SRB_InformationSetupList2
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_UM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 1
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 1
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . . . . . . . (TimerRST)timerRST = 9
. . . . . . . . . . . . . (MaxRST)max_RST = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 2
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 2
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . . . . . . . (TimerRST)timerRST = 9
. . . . . . . . . . . . . (MaxRST)max_RST = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 3
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 3
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . . . . . . . (TimerRST)timerRST = 9
. . . . . . . . . . . . . (MaxRST)max_RST = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 4
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 4
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . UL_CommonTransChInfo
. . . . . . . . TFC_Subset
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . TFCS
. . . . . . . . . . . ExplicitTFCS_Configuration
. . . . . . . . . . . . TFCS_ReconfAdd
. . . . . . . . . . . . . ctfcSize
. . . . . . . . . . . . . . ctfc2Bit
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . . . . . . . (IntegerType)ctfc2 = 0
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . . . . . . . (IntegerType)ctfc2 = 1
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 11
. . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . UL_AddReconfTransChInfoList
. . . . . . . . UL_AddReconfTransChInformation
. . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType = 0
. . . . . . . . . (IntegerType)transportChannelIdentity = 5
. . . . . . . . . TransportFormatSet
. . . . . . . . . . DedicatedTransChTFS
. . . . . . . . . . . tti
. . . . . . . . . . . . DedicatedDynamicTF_InfoList
. . . . . . . . . . . . . DedicatedDynamicTF_Info
. . . . . . . . . . . . . . rlc_Size
. . . . . . . . . . . . . . . BitModeRLC_SizeInfo
. . . . . . . . . . . . . . . . sizeType2
. . . . . . . . . . . . . . . . . (IntegerType)part1 = 2
. . . . . . . . . . . . . . . . . (IntegerType)part2 = -
. . . . . . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . LogicalChannelList
. . . . . . . . . . . SemistaticTF_Information
. . . . . . . . . . . . ChannelCodingType
. . . . . . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . . . . . (IntegerType)rateMatchingAttribute = 192
. . . . . . . . . . . . (CRC_Size)crc_Size = 3
. . . . . . . DL_CommonTransChInfo
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . dl_Parameters
. . . . . . . DL_AddReconfTransChInfoList
. . . . . . . . DL_AddReconfTransChInformation
. . . . . . . . . (DL_TrCH_Type)dl_TransportChannelType = 0
. . . . . . . . . (IntegerType)dl_transportChannelIdentity = 10
. . . . . . . . . tfs_SignallingMode
. . . . . . . . . . UL_TransportChannelIdentity
. . . . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType = 0
. . . . . . . . . . . (IntegerType)ul_TransportChannelIdentity = 5
. . . . . . . . . QualityTarget
. . . . . . . . . . (IntegerType)bler_QualityValue = -20
. . . . . . . . . TM_SignallingInfo
. . . . . . . FrequencyInfo
. . . . . . . (IntegerType)maxAllowedUL_TX_Power = -
. . . . . . . UL_ChannelRequirement
. . . . . . . . UL_DPCH_Info
. . . . . . . . . UL_DPCH_PowerControlInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (IntegerType)dpcch_PowerOffset = -40
. . . . . . . . . . . (IntegerType)pc_Preamble = 1
. . . . . . . . . . . (IntegerType)sRB_delay = 7
. . . . . . . . . . . PowerControlAlgorithm
. . . . . . . . . . . . (IntegerType)algorithm1 = 1
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (ScramblingCodeType)scramblingCodeType = 1
. . . . . . . . . . . (IntegerType)scramblingCode = 0
. . . . . . . . . . . (IntegerType)numberOfDPDCH = -
. . . . . . . . . . . (SpreadingFactor)spreadingFactor = 4
. . . . . . . . . . . (BooleanType)tfci_Existence = TRUE
. . . . . . . . . . . (IntegerType)numberOfFBI_Bits = -
. . . . . . . . . . . (PuncturingLimit)puncturingLimit = 15
. . . . . . . DL_CommonInformation
. . . . . . . . DL_DPCH_InfoCommon
. . . . . . . . . cfnHandling
. . . . . . . . . . initialise
. . . . . . . . . . . (IntegerType)cfntargetsfnframeoffset = -
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . DL_DPCH_PowerControlInfo
. . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . (DPC_Mode)dpc_Mode = 0
. . . . . . . . . . . (IntegerType)powerOffsetPilot_pdpdch = 0
. . . . . . . . . . . Dl_rate_matching_restriction
. . . . . . . . . . . SF512_AndPilot
. . . . . . . . . . . . (PilotBits128)sfd128 = 0
. . . . . . . . . . . (PositionFixedOrFlexible)positionFixedOrFlexible = 0
. . . . . . . . . . . (BooleanType)tfci_Existence = FALSE
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . (IntegerType)defaultDPCH_OffsetValue = 0
. . . . . . . . . . DPCH_CompressedModeInfo
. . . . . . . . . . (TX_DiversityMode)tx_DiversityMode = 0
. . . . . . . . . . SSDT_Information
. . . . . . . DL_InformationPerRL_List
. . . . . . . . DL_InformationPerRL
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . PrimaryCPICH_Info
. . . . . . . . . . . . (IntegerType)primaryScramblingCode = 100
. . . . . . . . . . . PDSCH_SHO_DCH_Info
. . . . . . . . . . . PDSCH_CodeMapping
. . . . . . . . . DL_DPCH_InfoPerRL
. . . . . . . . . . fdd
. . . . . . . . . . . (PCPICH_UsageForChannelEst)pCPICH_UsageForChannelEst = 0
. . . . . . . . . . . (IntegerType)dpch_FrameOffset = 0
. . . . . . . . . . . SecondaryCPICH_Info
. . . . . . . . . . . DL_ChannelisationCodeList
. . . . . . . . . . . . DL_ChannelisationCode
. . . . . . . . . . . . . (IntegerType)secondaryScramblingCode = 1
. . . . . . . . . . . . . SF512_AndCodeNumber
. . . . . . . . . . . . . . (IntegerType)sf128 = 0
. . . . . . . . . . . . . (ScramblingCodeChange)scramblingCodeChange = 1
. . . . . . . . . . . (IntegerType)tpc_CombinationIndex = 0
. . . . . . . . . . . (SSDT_CellIdentity)ssdt_CellIdentity = -
. . . . . . . . . . . (ClosedLoopTimingAdjMode)closedLoopTimingAdjMode = -
. . . . . . . . . SCCPCH_InfoForFACH
. . . . . . laterNonCriticalExtensions
. (BooleanType)specialLI = TRUE
- Constraint:
cas_RRC_ConnSetup
- BinaryMessage:
30 78 02 01 00 02 01 00 30 e7 22 46 8a cf 00 02 01 00 01 00 04 00 00 4d 82 69 3a 10 10 89 0d 42 00 02 81 9e 8e 46 c9 ce 7c 9c 4e 74 20 a5 12 3a 8c 00 15 13 3d 1c 8d 93 9c f9 38 9c e8 42 52 24 b5 28 00 4a 46 7a 39 1b 27 39 f2 71 39 d0 86 b4 49 ea 70 00 d4 c8 00 06 25 2b f0 02 00 08 82 23 bf 66 08 98 95 a5 47 a2 00 00 01 3f 90 0a 14 00 02 06 40 00 0c 28 08 01 01 ff

- No.: 807
- Timestamp: 20:48:38:831_0
- RFN: 1087
- Chip: 32256
- Event: Start Timer
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 3
- Message Structure:
no details available
- Constraint:
t_WaitMS (13500 Ms)
- BinaryMessage:

- No.: 812
- Timestamp: 20:48:39:071_0
- RFN: 1111
- Chip: 32000
- Event: Receive
- PCO: CPHY
- Message: CPHY_Sync_IND
- Source: RRC_Def1 LINE 13
- Message Structure:
CPHY_Sync_IND
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_SyncInd
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 813
- Timestamp: 20:48:39:071_1
- RFN: 1111
- Chip: 33792
- Event: Cancel Timer
- Source: RRC_Def1 LINE 13
- Message Structure:
no details available
- Constraint:
t_T312
- BinaryMessage:

- No.: 814
- Timestamp: 20:48:39:072_0
- RFN: 1111
- Chip: 35840
- Event: Default
- Source: RRC_Def1 LINE 0
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 815
- Timestamp: 20:48:39:072_1
- RFN: 1111
- Chip: 36608
- Event: Default
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 820
- Timestamp: 20:48:39:187_0
- RFN: 1123
- Chip: 13824
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_IND
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
RLC_AM_DATA_IND
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. IntegrityResult
. . (IntegrityStatus)integrityUsed = 0
. aM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode = 0
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . UL_DCCH_MessageType
. . . . RRCConnectionSetupComplete
. . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . STARTList
. . . . . . STARTSingle
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity = 1
. . . . . . . (BitStringType)start_Value[20] = "00000000000000000100"
. . . . . . STARTSingle
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity = 0
. . . . . . . (BitStringType)start_Value[20] = "00000000000000000010"
. . . . . UE_RadioAccessCapability
. . . . . . (AccessStratumReleaseIndicator)accessStratumReleaseIndicator = 0
. . . . . . PDCP_Capability
. . . . . . . (BooleanType)losslessSRNS_RelocationSupport = FALSE
. . . . . . . supportForRfc2507
. . . . . . RLC_Capability
. . . . . . . (TotalRLC_AM_BufferSize)totalRLC_AM_BufferSize = 2
. . . . . . . (MaximumRLC_WindowSize)maximumRLC_WindowSize = 0
. . . . . . . (MaximumAM_EntityNumberRLC_Cap)maximumAM_EntityNumber = 3
. . . . . . TransportChannelCapability
. . . . . . . DL_TransChCapability
. . . . . . . . (MaxNoBits)maxNoBitsReceived = 4
. . . . . . . . (MaxNoBits)maxConvCodeBitsReceived = 1
. . . . . . . . TurboSupport
. . . . . . . . . (MaxNoBits)supported = 4
. . . . . . . . (MaxSimultaneousTransChsDL)maxSimultaneousTransChs = 1
. . . . . . . . (IntegerType)maxSimultaneousCCTrCH_Count = 1
. . . . . . . . (MaxTransportBlocksDL)maxReceivedTransportBlocks = 2
. . . . . . . . (MaxNumberOfTFC_DL)maxNumberOfTFC = 4
. . . . . . . . (MaxNumberOfTF)maxNumberOfTF = 1
. . . . . . . UL_TransChCapability
. . . . . . . . (MaxNoBits)maxNoBitsTransmitted = 3
. . . . . . . . (MaxNoBits)maxConvCodeBitsTransmitted = 1
. . . . . . . . TurboSupport
. . . . . . . . . (MaxNoBits)supported = 3
. . . . . . . . (MaxSimultaneousTransChsUL)maxSimultaneousTransChs = 2
. . . . . . . . modeSpecificInfo
. . . . . . . . (MaxTransportBlocksUL)maxTransmittedBlocks = 2
. . . . . . . . (MaxNumberOfTFC_UL)maxNumberOfTFC = 3
. . . . . . . . (MaxNumberOfTF)maxNumberOfTF = 0
. . . . . . RF_Capability
. . . . . . . fddRF_Capability
. . . . . . . . (IntegerType)ue_PowerClass = 4
. . . . . . . . (TxRxFrequencySeparation)txRxFrequencySeparation = 0
. . . . . . . tddRF_Capability
. . . . . . . . (IntegerType)ue_PowerClass = 0
. . . . . . . . (RadioFrequencyBandTDDList)radioFrequencyTDDBandList = 0
. . . . . . . . (ChipRateCapability)chipRateCapability = 0
. . . . . . PhysicalChannelCapability
. . . . . . . fddPhysChCapability
. . . . . . . . DL_PhysChCapabilityFDD
. . . . . . . . . (IntegerType)maxNoDPCH_PDSCH_Codes = 3
. . . . . . . . . (MaxNoPhysChBitsReceived)maxNoPhysChBitsReceived = 6
. . . . . . . . . (BooleanType)supportForSF_512 = FALSE
. . . . . . . . . (BooleanType)supportOfPDSCH = FALSE
. . . . . . . . . SimultaneousSCCPCH_DPCH_Reception
. . . . . . . . UL_PhysChCapabilityFDD
. . . . . . . . . (MaxNoDPDCH_BitsTransmitted)maxNoDPDCH_BitsTransmitted = 2
. . . . . . . . . (BooleanType)supportOfPCPCH = FALSE
. . . . . . . tddPhysChCapability
. . . . . . . . DL_PhysChCapabilityTDD
. . . . . . . . . (IntegerType)maxTS_PerFrame = 0
. . . . . . . . . (IntegerType)maxPhysChPerFrame = 0
. . . . . . . . . (MinimumSF_DL)minimumSF = 0
. . . . . . . . . (BooleanType)supportOfPDSCH = FALSE
. . . . . . . . . (IntegerType)maxPhysChPerTS = 0
. . . . . . . . UL_PhysChCapabilityTDD
. . . . . . . . . (IntegerType)maxTS_PerFrame = 0
. . . . . . . . . (MaxPhysChPerTimeslot)maxPhysChPerTimeslot = 0
. . . . . . . . . (MinimumSF_UL)minimumSF = 0
. . . . . . . . . (BooleanType)supportOfPUSCH = FALSE
. . . . . . UE_MultiModeRAT_Capability
. . . . . . . MultiRAT_Capability
. . . . . . . . (BooleanType)supportOfGSM = TRUE
. . . . . . . . (BooleanType)supportOfMulticarrier = FALSE
. . . . . . . (MultiModeCapability)multiModeCapability = 1
. . . . . . SecurityCapability
. . . . . . . (BitStringType)cipheringAlgorithmCap[16] = '0000000000000011'B
. . . . . . . (BitStringType)integrityProtectionAlgorithmCap[16] = '0000000000000010'B
. . . . . . UE_Positioning_Capability
. . . . . . . (BooleanType)standaloneLocMethodsSupported = FALSE
. . . . . . . (BooleanType)ue_BasedOTDOA_Supported = FALSE
. . . . . . . (NetworkAssistedGPS_Supported)networkAssistedGPS_Supported = 3
. . . . . . . (BooleanType)supportForUE_GPS_TimingOfCellFrames = FALSE
. . . . . . . (BooleanType)supportForIPDL = FALSE
. . . . . . MeasurementCapability
. . . . . . . CompressedModeMeasCapability
. . . . . . . . (BooleanType)fdd_Measurements = TRUE
. . . . . . . . (BooleanType)tdd_Measurements = FALSE
. . . . . . . . GSM_Measurements
. . . . . . . . . (BooleanType)gsm900 = TRUE
. . . . . . . . . (BooleanType)dcs1800 = TRUE
. . . . . . . . . (BooleanType)gsm1900 = FALSE
. . . . . . . . (BooleanType)multiCarrierMeasurements = FALSE
. . . . . . . CompressedModeMeasCapability
. . . . . . . . (BooleanType)fdd_Measurements = TRUE
. . . . . . . . (BooleanType)tdd_Measurements = FALSE
. . . . . . . . GSM_Measurements
. . . . . . . . . (BooleanType)gsm900 = TRUE
. . . . . . . . . (BooleanType)dcs1800 = TRUE
. . . . . . . . . (BooleanType)gsm1900 = FALSE
. . . . . . . . (BooleanType)multiCarrierMeasurements = FALSE
. . . . . v370NonCriticalExtensions
. . . . . . RRCConnectionSetupComplete_v370ext
. . . . . . . UE_RadioAccessCapability_v370ext
. . . . . . v380NonCriticalExtensions
. . . . . . . RRCConnectionSetupComplete_v380ext_IEs
. . . . . . . . UE_RadioAccessCapability_v380ext
. . . . . . . . . UE_PositioningCapabilityExt_v380
. . . . . . . . . . (BooleanType)rx_tx_TimeDifferenceType2Capable = FALSE
. . . . . . . . DL_PhysChCapabilityFDD_v380ext
. . . . . . . . . (SupportOfDedicatedPilotsForChEstimation)supportOfDedicatedPilotsForChEstimation = 0
. . . . . . . v3a0NonCriticalExtensions
. . . . . . . . RRCConnectionSetupComplete_v3a0ext_IEs
. . . . . . . . . UE_RadioAccessCapability_v3a0ext
. . . . . . . . . . UE_PositioningCapabilityExt_v3a0
. . . . . . . . . . . (UE_PositioningCapabilityExt_v3a0_list_0)validity_CellPCH_UraPCH = 0
. . . . . . . . laterNonCriticalExtensions
. . . . . . . . . (BitStringType)rrcConnectionSetupComplete_r3_add_ext = 0
. . . . . . . . . nonCriticalExtensions
- Constraint:
car_RRC_ConnSetupCmpl
- BinaryMessage:
30 27 02 01 ff 02 01 02 0a 05 01 00 00 00 00 4a 0c 00 01 00 00 05 11 a0 d1 04 84 c6 68 46 2c 93 02 48 00 18 00 11 8f 8f 80

- No.: 821
- Timestamp: 20:48:39:198_0
- RFN: 1124
- Chip: 17408
- Event: Cancel Timer
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
t_WaitMS
- BinaryMessage:

- No.: 822
- Timestamp: 20:48:39:198_1
- RFN: 1124
- Chip: 18176
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 836
- Timestamp: 20:48:39:204_0
- RFN: 1125
- Chip: 2816
- Event: Send
- PCO: CMAC
- Message: CMAC_SecurityMode_Config_REQ
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 1
- Message Structure:
CMAC_SecurityMode_Config_REQ
. (IntegerType)cellId = 0
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity = 1
. . (BitStringType)startValue[20] = "00000000000000000100"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = -
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CMAC_SecurityModeCfgReq
- BinaryMessage:
30 0e 02 01 00 30 09 0a 01 01 03 04 04 00 00 40

- No.: 837
- Timestamp: 20:48:39:206_0
- RFN: 1125
- Chip: 8960
- Event: Receive
- PCO: CMAC
- Message: CMAC_SecurityMode_Config_CNF
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 2
- Message Structure:
CMAC_SecurityMode_Config_CNF
. (IntegerType)cellId = 0
- Constraint:
ca_CMAC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 00

- No.: 838
- Timestamp: 20:48:39:207_0
- RFN: 1125
- Chip: 16384
- Event: Send
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_REQ
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 3
- Message Structure:
CRLC_SecurityMode_Config_REQ
. (IntegerType)cellId = -1
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity = 1
. . (BitStringType)startValue[20] = "00000000000000000100"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = -
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CRLC_SecurityModeCfgReq
- BinaryMessage:
30 0e 02 01 ff 30 09 0a 01 01 03 04 04 00 00 40

- No.: 839
- Timestamp: 20:48:39:209_0
- RFN: 1125
- Chip: 22272
- Event: Receive
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_CNF
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 4
- Message Structure:
CRLC_SecurityMode_Config_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 853
- Timestamp: 20:48:39:214_0
- RFN: 1126
- Chip: 3072
- Event: Send
- PCO: CMAC
- Message: CMAC_SecurityMode_Config_REQ
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 1
- Message Structure:
CMAC_SecurityMode_Config_REQ
. (IntegerType)cellId = 0
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity = 0
. . (BitStringType)startValue[20] = "00000000000000000010"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = -
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CMAC_SecurityModeCfgReq
- BinaryMessage:
30 0e 02 01 00 30 09 0a 01 00 03 04 04 00 00 20

- No.: 854
- Timestamp: 20:48:39:216_0
- RFN: 1126
- Chip: 9216
- Event: Receive
- PCO: CMAC
- Message: CMAC_SecurityMode_Config_CNF
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 2
- Message Structure:
CMAC_SecurityMode_Config_CNF
. (IntegerType)cellId = 0
- Constraint:
ca_CMAC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 00

- No.: 855
- Timestamp: 20:48:39:217_0
- RFN: 1126
- Chip: 16384
- Event: Send
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_REQ
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 3
- Message Structure:
CRLC_SecurityMode_Config_REQ
. (IntegerType)cellId = -1
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity = 0
. . (BitStringType)startValue[20] = "00000000000000000010"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = -
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CRLC_SecurityModeCfgReq
- BinaryMessage:
30 0e 02 01 ff 30 09 0a 01 00 03 04 04 00 00 20

- No.: 856
- Timestamp: 20:48:39:219_0
- RFN: 1126
- Chip: 22272
- Event: Receive
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_CNF
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 4
- Message Structure:
CRLC_SecurityMode_Config_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 863
- Timestamp: 20:48:39:229_0
- RFN: 1127
- Chip: 23296
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_GMM_IdleUpdated:lt_IdleUpdated_NMO_II LINE 3
- Message Structure:
RRC_DataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain = 0
. (START_Value)start[20] = '00000000000000000010'B
. LOCATIONUPDATINGREQUEST
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)mMProtocolDiscriminator[4] = '0101'B
. . (MsgType)msgType[8] = '00001000'B
. . CiphKeySeqNum
. . . (B1)spare1[1] = '0'B
. . . (KeySeq)keySeq[3] = '000'B
. . LocUpdType
. . . (B1)fOR[1] = '0'B
. . . (B1)spare1[1] = '0'B
. . . (B2)lUT[2] = '10'B
. . LocAreaId_v
. . . (OctetStringType)plmn[3] = '00F110'O
. . . (OctetStringType)lac[2] = '0001'O
. . MS_Clsmk1
. . . (B1)spare1[1] = '0'B
. . . (B2)revLvl[2] = '10'B
. . . (B1)eSIND[1] = '0'B
. . . (B1)a5_1[1] = '1'B
. . . (B3)rFPwrCap[3] = '111'B
. . MS_Identity_lv
. . . (Length)iel[1] = '05'O
. . . (B4)iDigit1[4] = '1111'B
. . . (B1)oddEvenInd[1] = '0'B
. . . (B3)typeOfId[3] = '100'B
. . . (OctetStringType)otherDigits[4] = '12345678'O
. . MS_Clsmk2
. . . (IEI8)iei[8] = '00110011'B
. . . (Length)iel[1] = '03'O
. . . (B1)spare1_1[1] = '0'B
. . . (B2)revLvl[2] = '10'B
. . . (B1)eSIND[1] = '0'B
. . . (B1)a5_1[1] = '1'B
. . . (B3)rFPwrCap[3] = '111'B
. . . (B1)spare1_2[1] = '0'B
. . . (B1)pSCap[1] = '0'B
. . . (B2)sSSI[2] = '01'B
. . . (B1)sMCap[1] = '1'B
. . . (B1)vBS[1] = '0'B
. . . (B1)vGCS[1] = '0'B
. . . (B1)fC[1] = '0'B
. . . (B1)cM3[1] = '1'B
. . . (B1)spare1_3[1] = '0'B
. . . (B1)lCSVA[1] = '0'B
. . . (B1)uCS2[1] = '0'B
. . . (B1)soLSA[1] = '0'B
. . . (B1)cMSP[1] = '0'B
. . . (B1)a5_3[1] = '0'B
. . . (B1)a5_2[1] = '0'B
- Constraint:
car_InitDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 00 03 04 04 00 00 20 05 08 02 00 f1 10 00 01 4f 05 f4 12 34 56 78 33 03 4f 18 80

- No.: 900
- Timestamp: 20:48:39:251_0
- RFN: 1129
- Chip: 29696
- Event: Send
- PCO: Dc
- Message: RRC_DataReq
- Source: ts_MM_Authentication LINE 2
- Message Structure:
RRC_DataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[-1] = -
. (SapId)sapId[1] = -
. (SS_CN_DomainIdentity)cN_Domain = 0
. AUTHENTICATIONREQUEST
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)mMProtocolDiscriminator[4] = '0101'B
. . (MsgType)msgType[8] = '00010010'B
. . (B4)spare4[4] = '0000'B
. . CiphKeySeqNum
. . . (B1)spare1[1] = '0'B
. . . (KeySeq)keySeq[3] = '000'B
. . (MM_RAND)rAND[128] = '01010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101'B
. . AUTN
. . . (IEI8)iei[8] = '00100000'B
. . . (Length)iel[1] = '10'O
. . . (BitStringType)aUTN[128] = '01010110010100010101000001010011010100100101110100000000000000000101010101010100010101110101011001010001010100000101001101010010'B
- Constraint:
ca_DataReq
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 00 05 12 00 55 55 55 55 55 55 55 55 55 55 55 55 55 55 55 55 20 10 56 51 50 53 52 5d 00 00 55 54 57 56 51 50 53 52

- No.: 904
- Timestamp: 20:48:39:888_0
- RFN: 1193
- Chip: 17664
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_MM_Authentication LINE 7
- Message Structure:
RRC_DataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain = 0
. (START_Value)start[0] = -
. AUTHENTICATIONRESPONSE
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)mMProtocolDiscriminator[4] = '0101'B
. . (MsgType)msgType[8] = '01010100'B
. . (AuthRsp)authRsp[32] = '01010101010101000101011101010110'B
. . AuthRspExt
- Constraint:
car_UplinkDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 00 05 54 55 54 57 56

- No.: 942
- Timestamp: 20:48:39:901_0
- RFN: 1194
- Chip: 33024
- Event: Send
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_REQ
- Source: ts_SS_DownloadSecurityKey:lt_DownloadKeyCRLC LINE 1
- Message Structure:
CRLC_SecurityMode_Config_REQ
. (IntegerType)cellId = -1
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity = 0
. . (BitStringType)startValue[20] = "00000000000000000000"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = '01010111010101100101000101010000010100110101001001011101010111000101111101011110010110010101100001011011010110100101010101010100'B
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CRLC_SecurityModeCfgReq
- BinaryMessage:
30 21 02 01 ff 30 1c 0a 01 00 03 04 04 00 00 00 03 11 00 57 56 51 50 53 52 5d 5c 5f 5e 59 58 5b 5a 55 54

- No.: 943
- Timestamp: 20:48:39:903_0
- RFN: 1195
- Chip: 1792
- Event: Receive
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_CNF
- Source: ts_SS_DownloadSecurityKey:lt_DownloadKeyCRLC LINE 2
- Message Structure:
CRLC_SecurityMode_Config_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 950
- Timestamp: 20:48:39:907_0
- RFN: 1195
- Chip: 14848
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 1
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
. (IntegerType)count_I_LSB_UL = -
. (IntegerType)count_I_LSB_DL = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 00 02 01 00 02 01 00

- No.: 951
- Timestamp: 20:48:39:909_0
- RFN: 1195
- Chip: 22016
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 2
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 00 02 01 00

- No.: 952
- Timestamp: 20:48:39:910_0
- RFN: 1195
- Chip: 29184
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 3
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. (IntegerType)count_I_LSB_UL = -
. (IntegerType)count_I_LSB_DL = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 01 02 01 00

- No.: 953
- Timestamp: 20:48:39:912_0
- RFN: 1195
- Chip: 36352
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 4
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 954
- Timestamp: 20:48:39:914_0
- RFN: 1196
- Chip: 5632
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 5
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. (IntegerType)count_I_LSB_UL = -
. (IntegerType)count_I_LSB_DL = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 02 02 01 00

- No.: 955
- Timestamp: 20:48:39:916_0
- RFN: 1196
- Chip: 12544
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 6
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 956
- Timestamp: 20:48:39:918_0
- RFN: 1196
- Chip: 19968
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 7
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
. (IntegerType)count_I_LSB_UL = -
. (IntegerType)count_I_LSB_DL = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 03 02 01 00

- No.: 957
- Timestamp: 20:48:39:920_0
- RFN: 1196
- Chip: 26624
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 8
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 958
- Timestamp: 20:48:39:922_0
- RFN: 1196
- Chip: 33792
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 9
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
. (IntegerType)count_I_LSB_UL = -
. (IntegerType)count_I_LSB_DL = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 04 02 01 00

- No.: 959
- Timestamp: 20:48:39:924_0
- RFN: 1197
- Chip: 4096
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 10
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 963
- Timestamp: 20:48:39:927_0
- RFN: 1197
- Chip: 15360
- Event: Send
- PCO: CRLC
- Message: CRLC_Integrity_Activate_REQ
- Source: ts_CRLC_DL_Integrity LINE 1
- Message Structure:
CRLC_Integrity_Activate_REQ
. (IntegerType)cellId = -1
. (CN_DomainIdentity)cn_DomainIdentity = 0
. IntegrityActivationInfo
. . IntegrityProtectionModeInfo
. . . IntegrityProtectionModeCommand
. . . . startIntegrityProtection
. . . . . (BitStringType)integrityProtInitNumber[32] = "00000000000000000000000000000001"
. . . (IntegrityProtectionAlgorithm)integrityProtectionAlgorithm = 0
- Constraint:
ca_CRLC_DL_IntegrityActivateReq
- BinaryMessage:
30 15 02 01 ff 0a 01 00 30 0d 30 30 07 03 05 00 00 00 00 01 0a 01 00

- No.: 964
- Timestamp: 20:48:39:928_0
- RFN: 1197
- Chip: 22016
- Event: Receive
- PCO: CRLC
- Message: CRLC_Integrity_Activate_CNF
- Source: ts_CRLC_DL_Integrity LINE 2
- Message Structure:
CRLC_Integrity_Activate_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_IntegrityActivateCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 971
- Timestamp: 20:48:39:932_0
- RFN: 1197
- Chip: 36864
- Event: Send
- PCO: CRLC
- Message: CRLC_Integrity_Activate_REQ
- Source: ts_RB2_UL_IntegrityActivate LINE 1
- Message Structure:
CRLC_Integrity_Activate_REQ
. (IntegerType)cellId = -1
. (CN_DomainIdentity)cn_DomainIdentity = 0
. IntegrityActivationInfo
. . IntegrityProtActivationInfoList
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity = 2
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
- Constraint:
ca_CRLC_UL_IntegrityActivateReq
- BinaryMessage:
30 10 02 01 ff 0a 01 00 30 08 30 06 02 01 02 02 01 00

- No.: 972
- Timestamp: 20:48:39:934_0
- RFN: 1198
- Chip: 4608
- Event: Receive
- PCO: CRLC
- Message: CRLC_Integrity_Activate_CNF
- Source: ts_RB2_UL_IntegrityActivate LINE 2
- Message Structure:
CRLC_Integrity_Activate_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_IntegrityActivateCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 978
- Timestamp: 20:48:39:940_0
- RFN: 1198
- Chip: 28672
- Event: Send
- PCO: AM
- Message: RLC_AM_DATA_REQ
- Source: ts_RRC_Security:lt_SendSecurityModeCommand LINE 7
- Message Structure:
RLC_AM_DATA_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. AmConfirmationRequest
. aM_message
. . DL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00000000000000000000000000000000"
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . DL_DCCH_MessageType
. . . . SecurityModeCommand
. . . . . r3
. . . . . . SecurityModeCommand_r3_IEs
. . . . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . . . SecurityCapability
. . . . . . . . (BitStringType)cipheringAlgorithmCap[16] = '0000000000000011'B
. . . . . . . . (BitStringType)integrityProtectionAlgorithmCap[16] = '0000000000000010'B
. . . . . . . CipheringModeInfo
. . . . . . . IntegrityProtectionModeInfo
. . . . . . . . IntegrityProtectionModeCommand
. . . . . . . . . startIntegrityProtection
. . . . . . . . . . (BitStringType)integrityProtInitNumber[32] = "00000000000000000000000000000001"
. . . . . . . . (IntegrityProtectionAlgorithm)integrityProtectionAlgorithm = 0
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity = 0
. . . . . . . InterRAT_UE_SecurityCapList
. . . . . . laterNonCriticalExtensions
- Constraint:
cas_RRC_SecModeCmd
- BinaryMessage:
30 17 02 01 ff 02 01 02 05 00 80 00 00 00 04 04 00 01 80 01 40 00 00 00 20

- No.: 984
- Timestamp: 20:48:40:066_0
- RFN: 1211
- Chip: 13824
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_IND
- Source: ts_RRC_Security:lt_StartSecurity_UE LINE 8
- Message Structure:
RLC_AM_DATA_IND
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. IntegrityResult
. . (IntegrityStatus)integrityUsed = 0
. aM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "10000001100000001110110111011101"
. . . . (IntegerType)rrc_MessageSequenceNumber = 1
. . . UL_DCCH_MessageType
. . . . SecurityModeComplete
. . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . IntegrityProtActivationInfo
. . . . . . RRC_MessageSequenceNumberList
. . . . . . . (IntegerType)_elem = 0
. . . . . . . (IntegerType)_elem = 0
. . . . . . . (IntegerType)_elem = 0
. . . . . . . (IntegerType)_elem = 0
. . . . . . . (IntegerType)_elem = 0
. . . . . laterNonCriticalExtensions
. . . . . . (BitStringType)securityModeComplete_r3_add_ext = 0
. . . . . . nonCriticalExtensions
- Constraint:
car_RRC_SecModeCmpl
- BinaryMessage:
30 12 02 01 ff 02 01 02 0a 01 00 c0 c0 76 ee 8d 21 00 00 00

- No.: 985
- Timestamp: 20:48:40:067_0
- RFN: 1211
- Chip: 17920
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_Security:lt_StartSecurity_UE LINE 8
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 987
- Timestamp: 20:48:40:071_0
- RFN: 1211
- Chip: 33024
- Event: Send
- PCO: CRLC
- Message: CRLC_Integrity_Activate_REQ
- Source: ts_CRLC_UL_Integrity LINE 1
- Message Structure:
CRLC_Integrity_Activate_REQ
. (IntegerType)cellId = -1
. (CN_DomainIdentity)cn_DomainIdentity = 0
. IntegrityActivationInfo
. . IntegrityProtActivationInfoList
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity = 0
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity = 1
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity = 3
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity = 4
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
- Constraint:
ca_CRLC_UL_IntegrityActivateReq
- BinaryMessage:
30 28 02 01 ff 0a 01 00 30 20 30 06 02 01 00 02 01 00 30 06 02 01 01 02 01 00 30 06 02 01 03 02 01 00 30 06 02 01 04 02 01 00

- No.: 988
- Timestamp: 20:48:40:073_0
- RFN: 1212
- Chip: 2560
- Event: Receive
- PCO: CRLC
- Message: CRLC_Integrity_Activate_CNF
- Source: ts_CRLC_UL_Integrity LINE 2
- Message Structure:
CRLC_Integrity_Activate_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_IntegrityActivateCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 995
- Timestamp: 20:48:40:078_0
- RFN: 1212
- Chip: 23040
- Event: Send
- PCO: Dc
- Message: RRC_DataReq
- Source: ts_GMM_IdleUpdated:lt_LocUpdAcc LINE 2
- Message Structure:
RRC_DataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[-1] = -
. (SapId)sapId[1] = -
. (SS_CN_DomainIdentity)cN_Domain = 0
. LOCATIONUPDATINGACCEPT
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)mMProtocolDiscriminator[4] = '0101'B
. . (MsgType)msgType[8] = '00000010'B
. . LocAreaId_v
. . . (OctetStringType)plmn[3] = '00F110'O
. . . (OctetStringType)lac[2] = '0001'O
. . MM_MS_Identity
. . . (IEI8)iei[8] = '00010111'B
. . . (Length)iel[1] = '05'O
. . . (B4)iDigit1[4] = '1111'B
. . . (B1)oddEvenInd[1] = '0'B
. . . (B3)typeOfId[3] = '100'B
. . . (OctetStringType)otherDigits[-1] = '12345678'O
. . (FollowOnProceed)followOnProceed[8] = '10100001'B
. . (CTSPerm)cTSPerm[8] = '10100010'B
. . PLMN_List
- Constraint:
ca_DataReq
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 00 05 02 00 f1 10 00 01 17 05 f4 12 34 56 78 a1 a2

- No.: 999
- Timestamp: 20:48:40:224_0
- RFN: 1227
- Chip: 5376
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_GMM_IdleUpdated:lt_LocUpdAcc LINE 3
- Message Structure:
RRC_DataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain = 0
. (START_Value)start[0] = -
. TMSIREALLOCATIONCOMPLETE
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)mMProtocolDiscriminator[4] = '0101'B
. . (MsgType)msgType[8] = '10011011'B
- Constraint:
car_UplinkDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 00 05 9b

- No.: 1013
- Timestamp: 20:48:40:228_3
- RFN: 1227
- Chip: 21504
- Event: Start Timer
- Source: ts_RRC_Delay LINE 1
- Message Structure:
no details available
- Constraint:
t_Dly (1000 Ms)
- BinaryMessage:

- No.: 1017
- Timestamp: 20:48:41:216_0
- RFN: 1326
- Chip: 12800
- Event: Timeout
- Source: ts_RRC_Delay LINE 2
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 1022
- Timestamp: 20:48:41:221_0
- RFN: 1326
- Chip: 33024
- Event: Send
- PCO: UM
- Message: RLC_UM_DATA_REQ
- Source: ts_RRC_ConnRel:lt_Send_RRC_ConnectionRelease LINE 3
- Message Structure:
RLC_UM_DATA_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. uM_message
. . DL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00000000000000000000000000000000"
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . DL_DCCH_MessageType
. . . . RRCConnectionRelease
. . . . . r3
. . . . . . RRCConnectionRelease_r3_IEs
. . . . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . . . (IntegerType)n_308 = 1
. . . . . . . (ReleaseCause)releaseCause = 0
. . . . . . . Rplmn_Information
. . . . . . laterNonCriticalExtensions
. (BooleanType)specialLI = FALSE
- Constraint:
cas_RRC_ConnRelDCCH
- BinaryMessage:
30 10 02 01 ff 02 01 01 80 00 00 00 03 c8 00 01 01 00

- No.: 1026
- Timestamp: 20:48:41:354_0
- RFN: 1340
- Chip: 7936
- Event: Receive
- PCO: UM
- Message: RLC_UM_DATA_IND
- Source: ts_RRC_ConnRel:lt_Send_RRC_ConnectionRelease LINE 4
- Message Structure:
RLC_UM_DATA_IND
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. IntegrityResult
. uM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "10101101101011101001000000111001"
. . . . (IntegerType)rrc_MessageSequenceNumber = 1
. . . UL_DCCH_MessageType
. . . . RRCConnectionReleaseComplete
. . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . FailureCauseWithProtErr
. . . . . laterNonCriticalExtensions
. . . . . . (BitStringType)rrcConnectionReleaseComplete_r3_add_ext = 0
. . . . . . nonCriticalExtensions
- Constraint:
car_RRC_ConnRelCmplUM
- BinaryMessage:
30 0c 02 01 ff 02 01 01 d6 d7 48 1c 8c 40

- No.: 1027
- Timestamp: 20:48:41:355_0
- RFN: 1340
- Chip: 11520
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ConnRel:lt_Send_RRC_ConnectionRelease LINE 4
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1030
- Timestamp: 20:48:41:357_0
- RFN: 1340
- Chip: 17664
- Event: Start Timer
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 1
- Message Structure:
no details available
- Constraint:
t_Dly (5000 Ms)
- BinaryMessage:

- No.: 1034
- Timestamp: 20:48:41:505_0
- RFN: 1355
- Chip: 6912
- Event: Receive
- PCO: UM
- Message: RLC_UM_DATA_IND
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 4
- Message Structure:
RLC_UM_DATA_IND
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. IntegrityResult
. uM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00011100010101000111110101101001"
. . . . (IntegerType)rrc_MessageSequenceNumber = 2
. . . UL_DCCH_MessageType
. . . . RRCConnectionReleaseComplete
. . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . FailureCauseWithProtErr
. . . . . laterNonCriticalExtensions
. . . . . . (BitStringType)rrcConnectionReleaseComplete_r3_add_ext = 0
. . . . . . nonCriticalExtensions
- Constraint:
car_RRC_ConnRelCmplUM
- BinaryMessage:
30 0c 02 01 ff 02 01 01 8e 2a 3e b4 94 40

- No.: 1035
- Timestamp: 20:48:41:506_0
- RFN: 1355
- Chip: 10752
- Event: Cancel Timer
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 4
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 1036
- Timestamp: 20:48:41:506_1
- RFN: 1355
- Chip: 11776
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 4
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1042
- Timestamp: 20:48:41:510_0
- RFN: 1355
- Chip: 26880
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 01 0a 01 00 05 00

- No.: 1046
- Timestamp: 20:48:41:516_0
- RFN: 1356
- Chip: 13056
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 1049
- Timestamp: 20:48:41:519_0
- RFN: 1356
- Chip: 24320
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 02 0a 01 00 05 00

- No.: 1053
- Timestamp: 20:48:41:527_0
- RFN: 1357
- Chip: 14848
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 1056
- Timestamp: 20:48:41:530_0
- RFN: 1357
- Chip: 26624
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 03 0a 01 00 05 00

- No.: 1060
- Timestamp: 20:48:41:537_0
- RFN: 1358
- Chip: 15616
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 1063
- Timestamp: 20:48:41:539_0
- RFN: 1358
- Chip: 25856
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 04 0a 01 00 05 00

- No.: 1067
- Timestamp: 20:48:41:552_0
- RFN: 1359
- Chip: 36096
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 1070
- Timestamp: 20:48:41:559_0
- RFN: 1360
- Chip: 24832
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 136
. . . . . UL_RLC_Mode
. . . . . . UL_UM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (NoExplicitDiscard)timerBasedNoExplicit = 9
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = 1
. . . . (IntegerType)dLlogicalChannelIdentity = 1
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_UM_Info
- BinaryMessage:
30 22 02 01 ff 02 01 01 0a 01 00 30 17 30 0d 05 00 30 09 02 02 00 88 30 03 0a 01 09 30 06 02 01 01 02 01 01

- No.: 1074
- Timestamp: 20:48:41:570_0
- RFN: 1361
- Chip: 28672
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 1075
- Timestamp: 20:48:41:579_0
- RFN: 1362
- Chip: 23808
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 3
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . (TimerEPC)timerEPC = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . (TimerRST)timerRST = 9
. . . . . . . (MaxRST)max_RST = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = 2
. . . . (IntegerType)dLlogicalChannelIdentity = 2
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 02 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 27 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 02 02 01 02

- No.: 1079
- Timestamp: 20:48:41:593_0
- RFN: 1364
- Chip: 1024
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 4
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 1080
- Timestamp: 20:48:41:601_0
- RFN: 1364
- Chip: 34816
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 5
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . (TimerEPC)timerEPC = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . (TimerRST)timerRST = 9
. . . . . . . (MaxRST)max_RST = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = 3
. . . . (IntegerType)dLlogicalChannelIdentity = 3
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 03 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 27 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 03 02 01 03

- No.: 1084
- Timestamp: 20:48:41:620_0
- RFN: 1366
- Chip: 28160
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 6
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 1085
- Timestamp: 20:48:41:629_0
- RFN: 1367
- Chip: 24064
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 7
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . (TimerEPC)timerEPC = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . (TimerRST)timerRST = 9
. . . . . . . (MaxRST)max_RST = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = 4
. . . . (IntegerType)dLlogicalChannelIdentity = 4
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 04 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 27 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 04 02 01 04

- No.: 1089
- Timestamp: 20:48:41:645_0
- RFN: 1369
- Chip: 9728
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 8
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 1112
- Timestamp: 20:48:41:654_1
- RFN: 1370
- Chip: 6656
- Event: Start Timer
- Source: ts_GMM_IdleUpdated:lt_HandleAttachRequest LINE 5
- Message Structure:
no details available
- Constraint:
t_WaitS (1 Sec)
- BinaryMessage:

- No.: 1116
- Timestamp: 20:48:42:660_0
- RFN: 1470
- Chip: 26880
- Event: Timeout
- Source: ts_GMM_IdleUpdated:lt_HandleAttachRequest LINE 6
- Message Structure:
no details available
- Constraint:
t_WaitS
- BinaryMessage:

- No.: 1118
- Timestamp: 20:48:42:661_0
- RFN: 1470
- Chip: 29440
- Event: Start Timer
- Source: ts_GMM_IdleUpdated:lt_HandleAttachRequest LINE 7
- Message Structure:
no details available
- Constraint:
t_WaitS (60 Sec)
- BinaryMessage:

- No.: 1120
- Timestamp: 20:48:42:663_0
- RFN: 1471
- Chip: 0
- Event: Send
- PCO: Ut
- Message: AT_CmdReq
- Source: ts_AT_TriggerGMM_Attach LINE 1
- Message Structure:
AT_CmdReq
. (IA5StringType)cmd[-1] = "AT+CGATT=1"
. (HexStringType)sMS_BlockMode[-1] = -
- Constraint:
ca_AT_CmdReq
- BinaryMessage:
41 54 2b 43 47 41 54 54 3d 31 3c 43 52 3e

- No.: 1124
- Timestamp: 20:48:43:785_0
- RFN: 1583
- Chip: 11008
- Event: Receive
- PCO: Ut
- Message: AT_CmdCnf
- Source: ts_AT_TriggerGMM_Attach LINE 2
- Message Structure:
AT_CmdCnf
. (BooleanType)result = TRUE
. (IA5StringType)resultString[18] = "OK"
. (HexStringType)sMS_BlockMode[0] = -
- Constraint:
ca_AT_CmdCnf
- BinaryMessage:
80 3c 43 52 3e 3c 4c 46 3e 4f 4b 3c 43 52 3e 3c 4c 46 3e

- No.: 1141
- Timestamp: 20:48:43:792_0
- RFN: 1583
- Chip: 36096
- Event: Receive
- PCO: CPHY
- Message: CPHY_Out_of_Sync_IND
- Source: RRC_DefConnEst LINE 7
- Message Structure:
CPHY_Out_of_Sync_IND
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_OutOfSyncInd
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 1142
- Timestamp: 20:48:43:792_1
- RFN: 1583
- Chip: 37888
- Event: Cancel Timer
- Source: RRC_DefConnEst LINE 7
- Message Structure:
no details available
- Constraint:
t_T312
- BinaryMessage:

- No.: 1143
- Timestamp: 20:48:43:793_0
- RFN: 1584
- Chip: 1536
- Event: Default
- Source: RRC_DefConnEst LINE 0
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1144
- Timestamp: 20:48:43:793_1
- RFN: 1584
- Chip: 2304
- Event: Default
- Source: ts_RRC_ConnEst:lt_RcvConnReq LINE 2
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1149
- Timestamp: 20:48:45:317_0
- RFN: 1736
- Chip: 15872
- Event: Receive
- PCO: TM
- Message: RLC_TR_DATA_IND
- Source: ts_RRC_ConnEst:lt_RcvConnReq LINE 2
- Message Structure:
RLC_TR_DATA_IND
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
. tM_message
. . UL_CCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode = 0
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . UL_CCCH_MessageType
. . . . RRCConnectionRequest
. . . . . InitialUE_Identity
. . . . . . TMSI_and_LAI_GSM_MAP
. . . . . . . (BitStringType)tmsi[32] = "00010010001101000101011001111000"
. . . . . . . LAI
. . . . . . . . PLMN_Identity
. . . . . . . . . MCC
. . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . (IntegerType)_elem = 1
. . . . . . . . . MNC
. . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . (IntegerType)_elem = 1
. . . . . . . . (BitStringType)lac[16] = '0000000000000001'B
. . . . . (EstablishmentCause)establishmentCause = 12
. . . . . (ProtocolErrorIndicator)protocolErrorIndicator = 0
. . . . . MeasuredResultsOnRACH
. . . . . . currentCell
. . . . . . . modeSpecificInfo
. . . . . . . . fdd
. . . . . . . . . measurementQuantity
. . . . . . . . . . (IntegerType)cpich_Ec_N0 = 0
. . . . . v3d0NonCriticalExtensions
. . . . . . RRCConnectionRequest_v3d0ext_IEs
. . . . . . . (BitStringType)uESpecificBehaviourInformation1idle = 0
. . . . . . nonCriticalExtensions
- Constraint:
car_RRC_ConnReq
- BinaryMessage:
30 11 02 01 00 02 01 00 21 12 34 56 78 00 10 08 00 0b 00

- No.: 1153
- Timestamp: 20:48:45:377_0
- RFN: 1742
- Chip: 18432
- Event: Send
- PCO: UM
- Message: RLC_UM_DATA_REQ
- Source: ts_RRC_ConnEst:lt_Send_ConnSetUp LINE 22
- Message Structure:
RLC_UM_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
. uM_message
. . DL_CCCH_Message
. . . IntegrityCheckInfo
. . . DL_CCCH_MessageType
. . . . RRCConnectionSetup
. . . . . r3
. . . . . . RRCConnectionSetup_r3_IEs
. . . . . . . InitialUE_Identity
. . . . . . . . TMSI_and_LAI_GSM_MAP
. . . . . . . . . (BitStringType)tmsi[32] = "00010010001101000101011001111000"
. . . . . . . . . LAI
. . . . . . . . . . PLMN_Identity
. . . . . . . . . . . MCC
. . . . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . . . (IntegerType)_elem = 1
. . . . . . . . . . . MNC
. . . . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . . . (IntegerType)_elem = 1
. . . . . . . . . . (BitStringType)lac[16] = '0000000000000001'B
. . . . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . . . (IntegerType)activationTime = -
. . . . . . . U_RNTI
. . . . . . . . (BitStringType)srnc_Identity[12] = "000000000001"
. . . . . . . . (BitStringType)s_RNTI[20] = "00000000000000000001"
. . . . . . . (BitStringType)new_c_RNTI[16] = -
. . . . . . . (RRC_StateIndicator)rrc_StateIndicator = 0
. . . . . . . (IntegerType)utran_DRX_CycleLengthCoeff = 9
. . . . . . . CapabilityUpdateRequirement
. . . . . . . . (BooleanType)ue_RadioCapabilityFDDUpdateRequirement = TRUE
. . . . . . . . (BooleanType)ue_RadioCapabilityTDDUpdateRequirement = FALSE
. . . . . . . . SystemSpecificCapUpdateReqList
. . . . . . . . . (SystemSpecificCapUpdateReq)_elem = 0
. . . . . . . SRB_InformationSetupList2
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_UM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 1
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 1
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . . . . . . . (TimerRST)timerRST = 9
. . . . . . . . . . . . . (MaxRST)max_RST = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 2
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 2
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . . . . . . . (TimerRST)timerRST = 9
. . . . . . . . . . . . . (MaxRST)max_RST = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 3
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 3
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . . . . . . . (TimerRST)timerRST = 9
. . . . . . . . . . . . . (MaxRST)max_RST = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 4
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 4
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . UL_CommonTransChInfo
. . . . . . . . TFC_Subset
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . TFCS
. . . . . . . . . . . ExplicitTFCS_Configuration
. . . . . . . . . . . . TFCS_ReconfAdd
. . . . . . . . . . . . . ctfcSize
. . . . . . . . . . . . . . ctfc2Bit
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . . . . . . . (IntegerType)ctfc2 = 0
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . . . . . . . (IntegerType)ctfc2 = 1
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 11
. . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . UL_AddReconfTransChInfoList
. . . . . . . . UL_AddReconfTransChInformation
. . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType = 0
. . . . . . . . . (IntegerType)transportChannelIdentity = 5
. . . . . . . . . TransportFormatSet
. . . . . . . . . . DedicatedTransChTFS
. . . . . . . . . . . tti
. . . . . . . . . . . . DedicatedDynamicTF_InfoList
. . . . . . . . . . . . . DedicatedDynamicTF_Info
. . . . . . . . . . . . . . rlc_Size
. . . . . . . . . . . . . . . BitModeRLC_SizeInfo
. . . . . . . . . . . . . . . . sizeType2
. . . . . . . . . . . . . . . . . (IntegerType)part1 = 2
. . . . . . . . . . . . . . . . . (IntegerType)part2 = -
. . . . . . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . LogicalChannelList
. . . . . . . . . . . SemistaticTF_Information
. . . . . . . . . . . . ChannelCodingType
. . . . . . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . . . . . (IntegerType)rateMatchingAttribute = 192
. . . . . . . . . . . . (CRC_Size)crc_Size = 3
. . . . . . . DL_CommonTransChInfo
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . dl_Parameters
. . . . . . . DL_AddReconfTransChInfoList
. . . . . . . . DL_AddReconfTransChInformation
. . . . . . . . . (DL_TrCH_Type)dl_TransportChannelType = 0
. . . . . . . . . (IntegerType)dl_transportChannelIdentity = 10
. . . . . . . . . tfs_SignallingMode
. . . . . . . . . . UL_TransportChannelIdentity
. . . . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType = 0
. . . . . . . . . . . (IntegerType)ul_TransportChannelIdentity = 5
. . . . . . . . . QualityTarget
. . . . . . . . . . (IntegerType)bler_QualityValue = -20
. . . . . . . . . TM_SignallingInfo
. . . . . . . FrequencyInfo
. . . . . . . (IntegerType)maxAllowedUL_TX_Power = -
. . . . . . . UL_ChannelRequirement
. . . . . . . . UL_DPCH_Info
. . . . . . . . . UL_DPCH_PowerControlInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (IntegerType)dpcch_PowerOffset = -40
. . . . . . . . . . . (IntegerType)pc_Preamble = 1
. . . . . . . . . . . (IntegerType)sRB_delay = 7
. . . . . . . . . . . PowerControlAlgorithm
. . . . . . . . . . . . (IntegerType)algorithm1 = 1
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (ScramblingCodeType)scramblingCodeType = 1
. . . . . . . . . . . (IntegerType)scramblingCode = 0
. . . . . . . . . . . (IntegerType)numberOfDPDCH = -
. . . . . . . . . . . (SpreadingFactor)spreadingFactor = 4
. . . . . . . . . . . (BooleanType)tfci_Existence = TRUE
. . . . . . . . . . . (IntegerType)numberOfFBI_Bits = -
. . . . . . . . . . . (PuncturingLimit)puncturingLimit = 15
. . . . . . . DL_CommonInformation
. . . . . . . . DL_DPCH_InfoCommon
. . . . . . . . . cfnHandling
. . . . . . . . . . initialise
. . . . . . . . . . . (IntegerType)cfntargetsfnframeoffset = -
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . DL_DPCH_PowerControlInfo
. . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . (DPC_Mode)dpc_Mode = 0
. . . . . . . . . . . (IntegerType)powerOffsetPilot_pdpdch = 0
. . . . . . . . . . . Dl_rate_matching_restriction
. . . . . . . . . . . SF512_AndPilot
. . . . . . . . . . . . (PilotBits128)sfd128 = 0
. . . . . . . . . . . (PositionFixedOrFlexible)positionFixedOrFlexible = 0
. . . . . . . . . . . (BooleanType)tfci_Existence = FALSE
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . (IntegerType)defaultDPCH_OffsetValue = 0
. . . . . . . . . . DPCH_CompressedModeInfo
. . . . . . . . . . (TX_DiversityMode)tx_DiversityMode = 0
. . . . . . . . . . SSDT_Information
. . . . . . . DL_InformationPerRL_List
. . . . . . . . DL_InformationPerRL
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . PrimaryCPICH_Info
. . . . . . . . . . . . (IntegerType)primaryScramblingCode = 100
. . . . . . . . . . . PDSCH_SHO_DCH_Info
. . . . . . . . . . . PDSCH_CodeMapping
. . . . . . . . . DL_DPCH_InfoPerRL
. . . . . . . . . . fdd
. . . . . . . . . . . (PCPICH_UsageForChannelEst)pCPICH_UsageForChannelEst = 0
. . . . . . . . . . . (IntegerType)dpch_FrameOffset = 0
. . . . . . . . . . . SecondaryCPICH_Info
. . . . . . . . . . . DL_ChannelisationCodeList
. . . . . . . . . . . . DL_ChannelisationCode
. . . . . . . . . . . . . (IntegerType)secondaryScramblingCode = 1
. . . . . . . . . . . . . SF512_AndCodeNumber
. . . . . . . . . . . . . . (IntegerType)sf128 = 0
. . . . . . . . . . . . . (ScramblingCodeChange)scramblingCodeChange = 1
. . . . . . . . . . . (IntegerType)tpc_CombinationIndex = 0
. . . . . . . . . . . (SSDT_CellIdentity)ssdt_CellIdentity = -
. . . . . . . . . . . (ClosedLoopTimingAdjMode)closedLoopTimingAdjMode = -
. . . . . . . . . SCCPCH_InfoForFACH
. . . . . . laterNonCriticalExtensions
. (BooleanType)specialLI = TRUE
- Constraint:
cas_RRC_ConnSetup
- BinaryMessage:
30 78 02 01 00 02 01 00 30 e7 22 46 8a cf 00 02 01 00 01 00 04 00 00 4d 82 69 3a 10 10 89 0d 42 00 02 81 9e 8e 46 c9 ce 7c 9c 4e 74 20 a5 12 3a 8c 00 15 13 3d 1c 8d 93 9c f9 38 9c e8 42 52 24 b5 28 00 4a 46 7a 39 1b 27 39 f2 71 39 d0 86 b4 49 ea 70 00 d4 c8 00 06 25 2b f0 02 00 08 82 23 bf 66 08 98 95 a5 47 a2 00 00 01 3f 90 0a 14 00 02 06 40 00 0c 28 08 01 01 ff

- No.: 1174
- Timestamp: 20:48:45:420_2
- RFN: 1746
- Chip: 30976
- Event: Start Timer
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 3
- Message Structure:
no details available
- Constraint:
t_WaitMS (13500 Ms)
- BinaryMessage:

- No.: 1179
- Timestamp: 20:48:45:631_0
- RFN: 1767
- Chip: 31744
- Event: Receive
- PCO: CPHY
- Message: CPHY_Sync_IND
- Source: RRC_Def1 LINE 13
- Message Structure:
CPHY_Sync_IND
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_SyncInd
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 1180
- Timestamp: 20:48:45:631_1
- RFN: 1767
- Chip: 33536
- Event: Cancel Timer
- Source: RRC_Def1 LINE 13
- Message Structure:
no details available
- Constraint:
t_T312
- BinaryMessage:

- No.: 1181
- Timestamp: 20:48:45:632_0
- RFN: 1767
- Chip: 35584
- Event: Default
- Source: RRC_Def1 LINE 0
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1182
- Timestamp: 20:48:45:632_1
- RFN: 1767
- Chip: 36096
- Event: Default
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1187
- Timestamp: 20:48:45:745_0
- RFN: 1779
- Chip: 12288
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_IND
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
RLC_AM_DATA_IND
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. IntegrityResult
. . (IntegrityStatus)integrityUsed = 0
. aM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode = 0
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . UL_DCCH_MessageType
. . . . RRCConnectionSetupComplete
. . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . STARTList
. . . . . . STARTSingle
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity = 1
. . . . . . . (BitStringType)start_Value[20] = "00000000000000000100"
. . . . . . STARTSingle
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity = 0
. . . . . . . (BitStringType)start_Value[20] = "00000000000000000010"
. . . . . UE_RadioAccessCapability
. . . . . . (AccessStratumReleaseIndicator)accessStratumReleaseIndicator = 0
. . . . . . PDCP_Capability
. . . . . . . (BooleanType)losslessSRNS_RelocationSupport = FALSE
. . . . . . . supportForRfc2507
. . . . . . RLC_Capability
. . . . . . . (TotalRLC_AM_BufferSize)totalRLC_AM_BufferSize = 2
. . . . . . . (MaximumRLC_WindowSize)maximumRLC_WindowSize = 0
. . . . . . . (MaximumAM_EntityNumberRLC_Cap)maximumAM_EntityNumber = 3
. . . . . . TransportChannelCapability
. . . . . . . DL_TransChCapability
. . . . . . . . (MaxNoBits)maxNoBitsReceived = 4
. . . . . . . . (MaxNoBits)maxConvCodeBitsReceived = 1
. . . . . . . . TurboSupport
. . . . . . . . . (MaxNoBits)supported = 4
. . . . . . . . (MaxSimultaneousTransChsDL)maxSimultaneousTransChs = 1
. . . . . . . . (IntegerType)maxSimultaneousCCTrCH_Count = 1
. . . . . . . . (MaxTransportBlocksDL)maxReceivedTransportBlocks = 2
. . . . . . . . (MaxNumberOfTFC_DL)maxNumberOfTFC = 4
. . . . . . . . (MaxNumberOfTF)maxNumberOfTF = 1
. . . . . . . UL_TransChCapability
. . . . . . . . (MaxNoBits)maxNoBitsTransmitted = 3
. . . . . . . . (MaxNoBits)maxConvCodeBitsTransmitted = 1
. . . . . . . . TurboSupport
. . . . . . . . . (MaxNoBits)supported = 3
. . . . . . . . (MaxSimultaneousTransChsUL)maxSimultaneousTransChs = 2
. . . . . . . . modeSpecificInfo
. . . . . . . . (MaxTransportBlocksUL)maxTransmittedBlocks = 2
. . . . . . . . (MaxNumberOfTFC_UL)maxNumberOfTFC = 3
. . . . . . . . (MaxNumberOfTF)maxNumberOfTF = 0
. . . . . . RF_Capability
. . . . . . . fddRF_Capability
. . . . . . . . (IntegerType)ue_PowerClass = 4
. . . . . . . . (TxRxFrequencySeparation)txRxFrequencySeparation = 0
. . . . . . . tddRF_Capability
. . . . . . . . (IntegerType)ue_PowerClass = 0
. . . . . . . . (RadioFrequencyBandTDDList)radioFrequencyTDDBandList = 0
. . . . . . . . (ChipRateCapability)chipRateCapability = 0
. . . . . . PhysicalChannelCapability
. . . . . . . fddPhysChCapability
. . . . . . . . DL_PhysChCapabilityFDD
. . . . . . . . . (IntegerType)maxNoDPCH_PDSCH_Codes = 3
. . . . . . . . . (MaxNoPhysChBitsReceived)maxNoPhysChBitsReceived = 6
. . . . . . . . . (BooleanType)supportForSF_512 = FALSE
. . . . . . . . . (BooleanType)supportOfPDSCH = FALSE
. . . . . . . . . SimultaneousSCCPCH_DPCH_Reception
. . . . . . . . UL_PhysChCapabilityFDD
. . . . . . . . . (MaxNoDPDCH_BitsTransmitted)maxNoDPDCH_BitsTransmitted = 2
. . . . . . . . . (BooleanType)supportOfPCPCH = FALSE
. . . . . . . tddPhysChCapability
. . . . . . . . DL_PhysChCapabilityTDD
. . . . . . . . . (IntegerType)maxTS_PerFrame = 0
. . . . . . . . . (IntegerType)maxPhysChPerFrame = 0
. . . . . . . . . (MinimumSF_DL)minimumSF = 0
. . . . . . . . . (BooleanType)supportOfPDSCH = FALSE
. . . . . . . . . (IntegerType)maxPhysChPerTS = 0
. . . . . . . . UL_PhysChCapabilityTDD
. . . . . . . . . (IntegerType)maxTS_PerFrame = 0
. . . . . . . . . (MaxPhysChPerTimeslot)maxPhysChPerTimeslot = 0
. . . . . . . . . (MinimumSF_UL)minimumSF = 0
. . . . . . . . . (BooleanType)supportOfPUSCH = FALSE
. . . . . . UE_MultiModeRAT_Capability
. . . . . . . MultiRAT_Capability
. . . . . . . . (BooleanType)supportOfGSM = TRUE
. . . . . . . . (BooleanType)supportOfMulticarrier = FALSE
. . . . . . . (MultiModeCapability)multiModeCapability = 1
. . . . . . SecurityCapability
. . . . . . . (BitStringType)cipheringAlgorithmCap[16] = '0000000000000011'B
. . . . . . . (BitStringType)integrityProtectionAlgorithmCap[16] = '0000000000000010'B
. . . . . . UE_Positioning_Capability
. . . . . . . (BooleanType)standaloneLocMethodsSupported = FALSE
. . . . . . . (BooleanType)ue_BasedOTDOA_Supported = FALSE
. . . . . . . (NetworkAssistedGPS_Supported)networkAssistedGPS_Supported = 3
. . . . . . . (BooleanType)supportForUE_GPS_TimingOfCellFrames = FALSE
. . . . . . . (BooleanType)supportForIPDL = FALSE
. . . . . . MeasurementCapability
. . . . . . . CompressedModeMeasCapability
. . . . . . . . (BooleanType)fdd_Measurements = TRUE
. . . . . . . . (BooleanType)tdd_Measurements = FALSE
. . . . . . . . GSM_Measurements
. . . . . . . . . (BooleanType)gsm900 = TRUE
. . . . . . . . . (BooleanType)dcs1800 = TRUE
. . . . . . . . . (BooleanType)gsm1900 = FALSE
. . . . . . . . (BooleanType)multiCarrierMeasurements = FALSE
. . . . . . . CompressedModeMeasCapability
. . . . . . . . (BooleanType)fdd_Measurements = TRUE
. . . . . . . . (BooleanType)tdd_Measurements = FALSE
. . . . . . . . GSM_Measurements
. . . . . . . . . (BooleanType)gsm900 = TRUE
. . . . . . . . . (BooleanType)dcs1800 = TRUE
. . . . . . . . . (BooleanType)gsm1900 = FALSE
. . . . . . . . (BooleanType)multiCarrierMeasurements = FALSE
. . . . . v370NonCriticalExtensions
. . . . . . RRCConnectionSetupComplete_v370ext
. . . . . . . UE_RadioAccessCapability_v370ext
. . . . . . v380NonCriticalExtensions
. . . . . . . RRCConnectionSetupComplete_v380ext_IEs
. . . . . . . . UE_RadioAccessCapability_v380ext
. . . . . . . . . UE_PositioningCapabilityExt_v380
. . . . . . . . . . (BooleanType)rx_tx_TimeDifferenceType2Capable = FALSE
. . . . . . . . DL_PhysChCapabilityFDD_v380ext
. . . . . . . . . (SupportOfDedicatedPilotsForChEstimation)supportOfDedicatedPilotsForChEstimation = 0
. . . . . . . v3a0NonCriticalExtensions
. . . . . . . . RRCConnectionSetupComplete_v3a0ext_IEs
. . . . . . . . . UE_RadioAccessCapability_v3a0ext
. . . . . . . . . . UE_PositioningCapabilityExt_v3a0
. . . . . . . . . . . (UE_PositioningCapabilityExt_v3a0_list_0)validity_CellPCH_UraPCH = 0
. . . . . . . . laterNonCriticalExtensions
. . . . . . . . . (BitStringType)rrcConnectionSetupComplete_r3_add_ext = 0
. . . . . . . . . nonCriticalExtensions
- Constraint:
car_RRC_ConnSetupCmpl
- BinaryMessage:
30 27 02 01 ff 02 01 02 0a 05 01 00 00 00 00 4a 0c 00 01 00 00 05 11 a0 d1 04 84 c6 68 46 2c 93 02 48 00 18 00 11 8f 8f 80

- No.: 1188
- Timestamp: 20:48:45:753_0
- RFN: 1780
- Chip: 4096
- Event: Cancel Timer
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
t_WaitMS
- BinaryMessage:

- No.: 1189
- Timestamp: 20:48:45:754_0
- RFN: 1780
- Chip: 5120
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1203
- Timestamp: 20:48:45:762_0
- RFN: 1780
- Chip: 37632
- Event: Send
- PCO: CMAC
- Message: CMAC_SecurityMode_Config_REQ
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 1
- Message Structure:
CMAC_SecurityMode_Config_REQ
. (IntegerType)cellId = 0
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity = 1
. . (BitStringType)startValue[20] = "00000000000000000100"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = -
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CMAC_SecurityModeCfgReq
- BinaryMessage:
30 0e 02 01 00 30 09 0a 01 01 03 04 04 00 00 40

- No.: 1204
- Timestamp: 20:48:45:764_0
- RFN: 1781
- Chip: 7680
- Event: Receive
- PCO: CMAC
- Message: CMAC_SecurityMode_Config_CNF
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 2
- Message Structure:
CMAC_SecurityMode_Config_CNF
. (IntegerType)cellId = 0
- Constraint:
ca_CMAC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 00

- No.: 1205
- Timestamp: 20:48:45:766_0
- RFN: 1781
- Chip: 14592
- Event: Send
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_REQ
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 3
- Message Structure:
CRLC_SecurityMode_Config_REQ
. (IntegerType)cellId = -1
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity = 1
. . (BitStringType)startValue[20] = "00000000000000000100"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = -
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CRLC_SecurityModeCfgReq
- BinaryMessage:
30 0e 02 01 ff 30 09 0a 01 01 03 04 04 00 00 40

- No.: 1206
- Timestamp: 20:48:45:769_0
- RFN: 1781
- Chip: 20992
- Event: Receive
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_CNF
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 4
- Message Structure:
CRLC_SecurityMode_Config_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1220
- Timestamp: 20:48:45:774_0
- RFN: 1782
- Chip: 2048
- Event: Send
- PCO: CMAC
- Message: CMAC_SecurityMode_Config_REQ
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 1
- Message Structure:
CMAC_SecurityMode_Config_REQ
. (IntegerType)cellId = 0
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity = 0
. . (BitStringType)startValue[20] = "00000000000000000010"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = -
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CMAC_SecurityModeCfgReq
- BinaryMessage:
30 0e 02 01 00 30 09 0a 01 00 03 04 04 00 00 20

- No.: 1221
- Timestamp: 20:48:45:775_0
- RFN: 1782
- Chip: 8192
- Event: Receive
- PCO: CMAC
- Message: CMAC_SecurityMode_Config_CNF
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 2
- Message Structure:
CMAC_SecurityMode_Config_CNF
. (IntegerType)cellId = 0
- Constraint:
ca_CMAC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 00

- No.: 1222
- Timestamp: 20:48:45:777_0
- RFN: 1782
- Chip: 15104
- Event: Send
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_REQ
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 3
- Message Structure:
CRLC_SecurityMode_Config_REQ
. (IntegerType)cellId = -1
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity = 0
. . (BitStringType)startValue[20] = "00000000000000000010"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = -
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CRLC_SecurityModeCfgReq
- BinaryMessage:
30 0e 02 01 ff 30 09 0a 01 00 03 04 04 00 00 20

- No.: 1223
- Timestamp: 20:48:45:779_0
- RFN: 1782
- Chip: 21760
- Event: Receive
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_CNF
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 4
- Message Structure:
CRLC_SecurityMode_Config_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1230
- Timestamp: 20:48:45:788_0
- RFN: 1783
- Chip: 18688
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_GMM_IdleUpdated:lt_HandleAttachRequest LINE 10
- Message Structure:
RRC_DataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. (START_Value)start[20] = '00000000000000000100'B
. ATTACHREQUEST
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)gMMProtocolDiscriminator[4] = '1000'B
. . (MsgType)msgType[8] = '00000001'B
. . MS_NetworkCap_lv
. . . (Length)iel[1] = '02'O
. . . (OctetStringType)value[2] = 'E540'O
. . CiphKeySeqNum
. . . (B1)spare1[1] = '0'B
. . . (KeySeq)keySeq[3] = '000'B
. . AttachType
. . . (B1)pre_for[1] = '0'B
. . . (B3)type[3] = '001'B
. . DRXparamter
. . . (B8)splitPGcycleCode[8] = '00000111'B
. . . (B4)cnDRXcoef[4] = '0000'B
. . . (B1)splitOnCCCH[1] = '0'B
. . . (B3)nonDRXtimer[3] = '010'B
. . MS_Identity_lv
. . . (Length)iel[1] = '05'O
. . . (B4)iDigit1[4] = '1111'B
. . . (B1)oddEvenInd[1] = '0'B
. . . (B3)typeOfId[3] = '100'B
. . . (OctetStringType)otherDigits[4] = '12345678'O
. . RAI_v
. . . (OctetStringType)plmn[3] = '00F110'O
. . . (OctetStringType)lac[2] = '0001'O
. . . (OctetStringType)rac[1] = '05'O
. . MSRadioAccessCap_lv
. . . (Length)iel[1] = '0A'O
. . . (OctetStringType)value[10] = '14F382334C03263CA060'O
. . PTMSI_Signature
. . . (IEI8)iei[8] = '00010111'B
. . . (OctetStringType)value[3] = -
. . GPRS_Timer
. . . (IEI8)iei[8] = '00010110'B
. . . (B3)unit[0] = -
. . . (B5)value[0] = -
. . TMSI_Status
. . . (IEI4)iei[0] = -
. . . (B3)spare3[0] = -
. . . (B1)flag[0] = -
- Constraint:
car_PS_InitDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 03 04 04 00 00 40 08 01 02 e5 40 01 07 02 05 f4 12 34 56 78 00 f1 10 00 01 05 0a 14 f3 82 33 4c 03 26 3c a0 60 17 16

- No.: 1231
- Timestamp: 20:48:45:793_0
- RFN: 1784
- Chip: 0
- Event: Cancel Timer
- Source: ts_GMM_IdleUpdated:lt_HandleAttachRequest LINE 10
- Message Structure:
no details available
- Constraint:
t_WaitS
- BinaryMessage:

- No.: 1268
- Timestamp: 20:48:45:809_0
- RFN: 1785
- Chip: 24320
- Event: Send
- PCO: Dc
- Message: RRC_DataReq
- Source: ts_GMM_Authentication LINE 2
- Message Structure:
RRC_DataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[-1] = -
. (SapId)sapId[1] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. AUTHENTICATIONANDCIPHERINGREQUEST
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)gMMProtocolDiscriminator[4] = '1000'B
. . (MsgType)msgType[8] = '00010010'B
. . IMEISVRequest
. . . (B1)spare1[1] = '0'B
. . . (B3)value[3] = '000'B
. . CiphAlgorithm
. . . (B1)spare1[1] = '0'B
. . . (B3)algorithm[3] = '001'B
. . AC_ReferenceNumber
. . . (B4)value[4] = '0011'B
. . ForceToStandby
. . . (B1)spare[1] = '0'B
. . . (B3)value[3] = '000'B
. . AuthenticationParamterRAND
. . . (IEI8)iei[8] = '00100001'B
. . . (BitStringType)randValue[128] = '01010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101'B
. . CiphKeySeqNum_tv
. . . (IEI4)iei[4] = '1000'B
. . . (B1)spare1[1] = '0'B
. . . (KeySeq)keySeq[3] = '000'B
. . GMM_AUTN
. . . (IEI8)iei[8] = '00101000'B
. . . (Length)iel[1] = '10'O
. . . (BitStringType)aUTN[128] = '01010110010100010101000001010011010100100101110100000000000000000101010101010100010101110101011001010001010100000101001101010010'B
- Constraint:
ca_PS_DataReq
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 08 12 01 30 21 55 55 55 55 55 55 55 55 55 55 55 55 55 55 55 55 80 28 10 56 51 50 53 52 5d 00 00 55 54 57 56 51 50 53 52

- No.: 1272
- Timestamp: 20:48:46:478_0
- RFN: 1852
- Chip: 21504
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_GMM_Authentication LINE 7
- Message Structure:
RRC_DataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. (START_Value)start[0] = -
. AUTHENTICATIONANDCIPHERINGRESPONSE
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)gMMProtocolDiscriminator[4] = '1000'B
. . (MsgType)msgType[8] = '00010011'B
. . (B4)spare4[4] = '0000'B
. . AC_ReferenceNumber
. . . (B4)value[4] = '0011'B
. . AuthRsp_tv
. . . (IEI8)iei[8] = '00100010'B
. . . (BitStringType)value[32] = '01010101010101000101011101010110'B
. . GMM_MS_Identity
. . AuthRspExt
- Constraint:
car_PS_UplinkDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 08 13 03 22 55 54 57 56

- No.: 1275
- Timestamp: 20:48:46:481_1
- RFN: 1852
- Chip: 30464
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_GMM_Authentication LINE 10
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1312
- Timestamp: 20:48:46:494_0
- RFN: 1854
- Chip: 3072
- Event: Send
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_REQ
- Source: ts_SS_DownloadSecurityKey:lt_DownloadKeyCRLC LINE 1
- Message Structure:
CRLC_SecurityMode_Config_REQ
. (IntegerType)cellId = -1
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity = 1
. . (BitStringType)startValue[20] = "00000000000000000000"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = '01010111010101100101000101010000010100110101001001011101010111000101111101011110010110010101100001011011010110100101010101010100'B
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CRLC_SecurityModeCfgReq
- BinaryMessage:
30 21 02 01 ff 30 1c 0a 01 01 03 04 04 00 00 00 03 11 00 57 56 51 50 53 52 5d 5c 5f 5e 59 58 5b 5a 55 54

- No.: 1313
- Timestamp: 20:48:46:495_0
- RFN: 1854
- Chip: 9984
- Event: Receive
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_CNF
- Source: ts_SS_DownloadSecurityKey:lt_DownloadKeyCRLC LINE 2
- Message Structure:
CRLC_SecurityMode_Config_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1320
- Timestamp: 20:48:46:499_0
- RFN: 1854
- Chip: 22016
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 1
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
. (IntegerType)count_I_LSB_UL = -
. (IntegerType)count_I_LSB_DL = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 00 02 01 00 02 01 00

- No.: 1321
- Timestamp: 20:48:46:501_0
- RFN: 1854
- Chip: 29952
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 2
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 00 02 01 00

- No.: 1322
- Timestamp: 20:48:46:502_0
- RFN: 1854
- Chip: 36864
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 3
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. (IntegerType)count_I_LSB_UL = -
. (IntegerType)count_I_LSB_DL = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 01 02 01 00

- No.: 1323
- Timestamp: 20:48:46:504_0
- RFN: 1855
- Chip: 5888
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 4
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 1324
- Timestamp: 20:48:46:506_0
- RFN: 1855
- Chip: 13312
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 5
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. (IntegerType)count_I_LSB_UL = -
. (IntegerType)count_I_LSB_DL = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 02 02 01 00

- No.: 1325
- Timestamp: 20:48:46:508_0
- RFN: 1855
- Chip: 20224
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 6
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 1326
- Timestamp: 20:48:46:510_0
- RFN: 1855
- Chip: 27136
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 7
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
. (IntegerType)count_I_LSB_UL = -
. (IntegerType)count_I_LSB_DL = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 03 02 01 00

- No.: 1327
- Timestamp: 20:48:46:512_0
- RFN: 1855
- Chip: 34304
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 8
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 1328
- Timestamp: 20:48:46:514_0
- RFN: 1856
- Chip: 3584
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 9
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
. (IntegerType)count_I_LSB_UL = -
. (IntegerType)count_I_LSB_DL = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 04 02 01 00

- No.: 1329
- Timestamp: 20:48:46:516_0
- RFN: 1856
- Chip: 10496
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 10
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 1333
- Timestamp: 20:48:46:518_0
- RFN: 1856
- Chip: 21504
- Event: Send
- PCO: CRLC
- Message: CRLC_Integrity_Activate_REQ
- Source: ts_CRLC_DL_Integrity LINE 1
- Message Structure:
CRLC_Integrity_Activate_REQ
. (IntegerType)cellId = -1
. (CN_DomainIdentity)cn_DomainIdentity = 1
. IntegrityActivationInfo
. . IntegrityProtectionModeInfo
. . . IntegrityProtectionModeCommand
. . . . startIntegrityProtection
. . . . . (BitStringType)integrityProtInitNumber[32] = "00000000000000000000000000000001"
. . . (IntegrityProtectionAlgorithm)integrityProtectionAlgorithm = 0
- Constraint:
ca_CRLC_DL_IntegrityActivateReq
- BinaryMessage:
30 15 02 01 ff 0a 01 01 30 0d 30 30 07 03 05 00 00 00 00 01 0a 01 00

- No.: 1334
- Timestamp: 20:48:46:520_0
- RFN: 1856
- Chip: 27648
- Event: Receive
- PCO: CRLC
- Message: CRLC_Integrity_Activate_CNF
- Source: ts_CRLC_DL_Integrity LINE 2
- Message Structure:
CRLC_Integrity_Activate_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_IntegrityActivateCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1341
- Timestamp: 20:48:46:524_0
- RFN: 1857
- Chip: 3840
- Event: Send
- PCO: CRLC
- Message: CRLC_Integrity_Activate_REQ
- Source: ts_RB2_UL_IntegrityActivate LINE 1
- Message Structure:
CRLC_Integrity_Activate_REQ
. (IntegerType)cellId = -1
. (CN_DomainIdentity)cn_DomainIdentity = 1
. IntegrityActivationInfo
. . IntegrityProtActivationInfoList
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity = 2
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
- Constraint:
ca_CRLC_UL_IntegrityActivateReq
- BinaryMessage:
30 10 02 01 ff 0a 01 01 30 08 30 06 02 01 02 02 01 00

- No.: 1342
- Timestamp: 20:48:46:525_0
- RFN: 1857
- Chip: 9984
- Event: Receive
- PCO: CRLC
- Message: CRLC_Integrity_Activate_CNF
- Source: ts_RB2_UL_IntegrityActivate LINE 2
- Message Structure:
CRLC_Integrity_Activate_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_IntegrityActivateCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1348
- Timestamp: 20:48:46:532_0
- RFN: 1857
- Chip: 33536
- Event: Send
- PCO: AM
- Message: RLC_AM_DATA_REQ
- Source: ts_RRC_Security:lt_SendSecurityModeCommand LINE 7
- Message Structure:
RLC_AM_DATA_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. AmConfirmationRequest
. aM_message
. . DL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00000000000000000000000000000000"
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . DL_DCCH_MessageType
. . . . SecurityModeCommand
. . . . . r3
. . . . . . SecurityModeCommand_r3_IEs
. . . . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . . . SecurityCapability
. . . . . . . . (BitStringType)cipheringAlgorithmCap[16] = '0000000000000011'B
. . . . . . . . (BitStringType)integrityProtectionAlgorithmCap[16] = '0000000000000010'B
. . . . . . . CipheringModeInfo
. . . . . . . IntegrityProtectionModeInfo
. . . . . . . . IntegrityProtectionModeCommand
. . . . . . . . . startIntegrityProtection
. . . . . . . . . . (BitStringType)integrityProtInitNumber[32] = "00000000000000000000000000000001"
. . . . . . . . (IntegrityProtectionAlgorithm)integrityProtectionAlgorithm = 0
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity = 1
. . . . . . . InterRAT_UE_SecurityCapList
. . . . . . laterNonCriticalExtensions
- Constraint:
cas_RRC_SecModeCmd
- BinaryMessage:
30 17 02 01 ff 02 01 02 05 00 80 00 00 00 04 04 00 01 80 01 40 00 00 00 30

- No.: 1354
- Timestamp: 20:48:46:666_0
- RFN: 1871
- Chip: 13312
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_IND
- Source: ts_RRC_Security:lt_StartSecurity_UE LINE 8
- Message Structure:
RLC_AM_DATA_IND
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. IntegrityResult
. . (IntegrityStatus)integrityUsed = 0
. aM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "10000001100000001110110111011101"
. . . . (IntegerType)rrc_MessageSequenceNumber = 1
. . . UL_DCCH_MessageType
. . . . SecurityModeComplete
. . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . IntegrityProtActivationInfo
. . . . . . RRC_MessageSequenceNumberList
. . . . . . . (IntegerType)_elem = 0
. . . . . . . (IntegerType)_elem = 0
. . . . . . . (IntegerType)_elem = 0
. . . . . . . (IntegerType)_elem = 0
. . . . . . . (IntegerType)_elem = 0
. . . . . laterNonCriticalExtensions
. . . . . . (BitStringType)securityModeComplete_r3_add_ext = 0
. . . . . . nonCriticalExtensions
- Constraint:
car_RRC_SecModeCmpl
- BinaryMessage:
30 12 02 01 ff 02 01 02 0a 01 00 c0 c0 76 ee 8d 21 00 00 00

- No.: 1355
- Timestamp: 20:48:46:667_0
- RFN: 1871
- Chip: 17152
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_Security:lt_StartSecurity_UE LINE 8
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1357
- Timestamp: 20:48:46:671_0
- RFN: 1871
- Chip: 33536
- Event: Send
- PCO: CRLC
- Message: CRLC_Integrity_Activate_REQ
- Source: ts_CRLC_UL_Integrity LINE 1
- Message Structure:
CRLC_Integrity_Activate_REQ
. (IntegerType)cellId = -1
. (CN_DomainIdentity)cn_DomainIdentity = 1
. IntegrityActivationInfo
. . IntegrityProtActivationInfoList
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity = 0
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity = 1
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity = 3
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity = 4
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
- Constraint:
ca_CRLC_UL_IntegrityActivateReq
- BinaryMessage:
30 28 02 01 ff 0a 01 01 30 20 30 06 02 01 00 02 01 00 30 06 02 01 01 02 01 00 30 06 02 01 03 02 01 00 30 06 02 01 04 02 01 00

- No.: 1358
- Timestamp: 20:48:46:673_0
- RFN: 1872
- Chip: 2304
- Event: Receive
- PCO: CRLC
- Message: CRLC_Integrity_Activate_CNF
- Source: ts_CRLC_UL_Integrity LINE 2
- Message Structure:
CRLC_Integrity_Activate_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_IntegrityActivateCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1368
- Timestamp: 20:48:46:681_0
- RFN: 1872
- Chip: 34048
- Event: Send
- PCO: Dc
- Message: RRC_DataReq
- Source: ts_GMM_IdleUpdated:lt_AttachAccept LINE 12
- Message Structure:
RRC_DataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[-1] = -
. (SapId)sapId[1] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. ATTACHACCEPT
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)gMMProtocolDiscriminator[4] = '1000'B
. . (MsgType)msgType[8] = '00000010'B
. . ForceToStandby
. . . (B1)spare[1] = '0'B
. . . (B3)value[3] = '000'B
. . AttachResult
. . . (B1)spare[1] = '0'B
. . . (B3)result[3] = '001'B
. . GPRS_Timer_v
. . . (B3)unit[3] = '111'B
. . . (B5)value[5] = '00000'B
. . (B4)spare[4] = '0000'B
. . RadioPriority_v
. . . (B1)spare[1] = '0'B
. . . (B3)value[3] = '100'B
. . RAI_v
. . . (OctetStringType)plmn[3] = '00F110'O
. . . (OctetStringType)lac[2] = '0001'O
. . . (OctetStringType)rac[1] = '05'O
. . PTMSI_Signature
. . . (IEI8)iei[8] = '00011001'B
. . . (OctetStringType)value[3] = 'AB1234'O
. . GPRS_Timer
. . GMM_MS_IdentityPTMSI
. . . (IEI8)iei[8] = '00011000'B
. . . (Length)iel[1] = '05'O
. . . (B4)iDigit1[4] = '1111'B
. . . (B1)oddEvenInd[1] = '0'B
. . . (B3)typeOfId[3] = '100'B
. . . (OctetStringType)otherDigits[-1] = '12345678'O
. . GMM_MS_Identity
. . GMM_Cause
. . GPRS_Timer
. . CellNotification
. . PLMN_List
- Constraint:
ca_PS_DataReq
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 08 02 01 e0 04 00 f1 10 00 01 05 19 ab 12 34 18 05 f4 12 34 56 78

- No.: 1372
- Timestamp: 20:48:46:824_0
- RFN: 1887
- Chip: 4864
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_GMM_IdleUpdated:lt_AttachAccept LINE 13
- Message Structure:
RRC_DataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. (START_Value)start[0] = -
. ATTACHCOMPLETE
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)gMMProtocolDiscriminator[4] = '1000'B
. . (MsgType)msgType[8] = '00000011'B
- Constraint:
car_PS_UplinkDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 08 03

- No.: 1383
- Timestamp: 20:48:46:828_0
- RFN: 1887
- Chip: 18176
- Event: Start Timer
- Source: ts_RRC_Delay LINE 1
- Message Structure:
no details available
- Constraint:
t_Dly (1000 Ms)
- BinaryMessage:

- No.: 1387
- Timestamp: 20:48:47:825_0
- RFN: 1987
- Chip: 9216
- Event: Timeout
- Source: ts_RRC_Delay LINE 2
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 1392
- Timestamp: 20:48:47:831_0
- RFN: 1987
- Chip: 30720
- Event: Send
- PCO: UM
- Message: RLC_UM_DATA_REQ
- Source: ts_RRC_ConnRel:lt_Send_RRC_ConnectionRelease LINE 3
- Message Structure:
RLC_UM_DATA_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. uM_message
. . DL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00000000000000000000000000000000"
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . DL_DCCH_MessageType
. . . . RRCConnectionRelease
. . . . . r3
. . . . . . RRCConnectionRelease_r3_IEs
. . . . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . . . (IntegerType)n_308 = 1
. . . . . . . (ReleaseCause)releaseCause = 0
. . . . . . . Rplmn_Information
. . . . . . laterNonCriticalExtensions
. (BooleanType)specialLI = FALSE
- Constraint:
cas_RRC_ConnRelDCCH
- BinaryMessage:
30 10 02 01 ff 02 01 01 80 00 00 00 03 c8 00 01 01 00

- No.: 1396
- Timestamp: 20:48:47:954_0
- RFN: 2000
- Chip: 7936
- Event: Receive
- PCO: UM
- Message: RLC_UM_DATA_IND
- Source: ts_RRC_ConnRel:lt_Send_RRC_ConnectionRelease LINE 4
- Message Structure:
RLC_UM_DATA_IND
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. IntegrityResult
. uM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "10101101101011101001000000111001"
. . . . (IntegerType)rrc_MessageSequenceNumber = 1
. . . UL_DCCH_MessageType
. . . . RRCConnectionReleaseComplete
. . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . FailureCauseWithProtErr
. . . . . laterNonCriticalExtensions
. . . . . . (BitStringType)rrcConnectionReleaseComplete_r3_add_ext = 0
. . . . . . nonCriticalExtensions
- Constraint:
car_RRC_ConnRelCmplUM
- BinaryMessage:
30 0c 02 01 ff 02 01 01 d6 d7 48 1c 8c 40

- No.: 1397
- Timestamp: 20:48:47:955_0
- RFN: 2000
- Chip: 11520
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ConnRel:lt_Send_RRC_ConnectionRelease LINE 4
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1400
- Timestamp: 20:48:47:957_1
- RFN: 2000
- Chip: 17920
- Event: Start Timer
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 1
- Message Structure:
no details available
- Constraint:
t_Dly (5000 Ms)
- BinaryMessage:

- No.: 1404
- Timestamp: 20:48:48:105_0
- RFN: 2015
- Chip: 7680
- Event: Receive
- PCO: UM
- Message: RLC_UM_DATA_IND
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 4
- Message Structure:
RLC_UM_DATA_IND
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. IntegrityResult
. uM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00011100010101000111110101101001"
. . . . (IntegerType)rrc_MessageSequenceNumber = 2
. . . UL_DCCH_MessageType
. . . . RRCConnectionReleaseComplete
. . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . FailureCauseWithProtErr
. . . . . laterNonCriticalExtensions
. . . . . . (BitStringType)rrcConnectionReleaseComplete_r3_add_ext = 0
. . . . . . nonCriticalExtensions
- Constraint:
car_RRC_ConnRelCmplUM
- BinaryMessage:
30 0c 02 01 ff 02 01 01 8e 2a 3e b4 94 40

- No.: 1405
- Timestamp: 20:48:48:106_0
- RFN: 2015
- Chip: 11776
- Event: Cancel Timer
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 4
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 1406
- Timestamp: 20:48:48:106_1
- RFN: 2015
- Chip: 12800
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ConnRel:lt_RptRcvConnRel LINE 4
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1412
- Timestamp: 20:48:48:110_0
- RFN: 2015
- Chip: 27136
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 01 0a 01 00 05 00

- No.: 1416
- Timestamp: 20:48:48:116_0
- RFN: 2016
- Chip: 12288
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 1419
- Timestamp: 20:48:48:119_0
- RFN: 2016
- Chip: 23296
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 02 0a 01 00 05 00

- No.: 1423
- Timestamp: 20:48:48:126_0
- RFN: 2017
- Chip: 12544
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 1426
- Timestamp: 20:48:48:129_0
- RFN: 2017
- Chip: 23808
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 03 0a 01 00 05 00

- No.: 1430
- Timestamp: 20:48:48:136_0
- RFN: 2018
- Chip: 13824
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 1433
- Timestamp: 20:48:48:139_0
- RFN: 2018
- Chip: 24832
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 04 0a 01 00 05 00

- No.: 1437
- Timestamp: 20:48:48:146_0
- RFN: 2019
- Chip: 13312
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 1440
- Timestamp: 20:48:48:153_0
- RFN: 2020
- Chip: 1024
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 136
. . . . . UL_RLC_Mode
. . . . . . UL_UM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (NoExplicitDiscard)timerBasedNoExplicit = 9
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = 1
. . . . (IntegerType)dLlogicalChannelIdentity = 1
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_UM_Info
- BinaryMessage:
30 22 02 01 ff 02 01 01 0a 01 00 30 17 30 0d 05 00 30 09 02 02 00 88 30 03 0a 01 09 30 06 02 01 01 02 01 01

- No.: 1444
- Timestamp: 20:48:48:163_0
- RFN: 2021
- Chip: 2816
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 1445
- Timestamp: 20:48:48:172_0
- RFN: 2021
- Chip: 35840
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 3
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . (TimerEPC)timerEPC = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . (TimerRST)timerRST = 9
. . . . . . . (MaxRST)max_RST = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = 2
. . . . (IntegerType)dLlogicalChannelIdentity = 2
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 02 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 27 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 02 02 01 02

- No.: 1449
- Timestamp: 20:48:48:186_0
- RFN: 2023
- Chip: 13312
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 4
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 1450
- Timestamp: 20:48:48:195_0
- RFN: 2024
- Chip: 8192
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 5
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . (TimerEPC)timerEPC = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . (TimerRST)timerRST = 9
. . . . . . . (MaxRST)max_RST = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = 3
. . . . (IntegerType)dLlogicalChannelIdentity = 3
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 03 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 27 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 03 02 01 03

- No.: 1454
- Timestamp: 20:48:48:210_0
- RFN: 2025
- Chip: 29440
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 6
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 1455
- Timestamp: 20:48:48:219_0
- RFN: 2026
- Chip: 25856
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 7
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . (TimerEPC)timerEPC = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . (TimerRST)timerRST = 9
. . . . . . . (MaxRST)max_RST = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = 4
. . . . (IntegerType)dLlogicalChannelIdentity = 4
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 04 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 27 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 04 02 01 04

- No.: 1459
- Timestamp: 20:48:48:239_0
- RFN: 2028
- Chip: 26624
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 8
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 1501
- Timestamp: 20:48:48:254_1
- RFN: 2030
- Chip: 6144
- Event: Start Timer
- Source: ts_RRC_Delay LINE 1
- Message Structure:
no details available
- Constraint:
t_Dly (5000 Ms)
- BinaryMessage:

- No.: 1503
- Timestamp: 20:48:48:257_0
- RFN: 2030
- Chip: 16640
- Event: Receive
- PCO: CPHY
- Message: CPHY_Out_of_Sync_IND
- Source: RRC_Def1 LINE 15
- Message Structure:
CPHY_Out_of_Sync_IND
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_OutOfSyncInd
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 1504
- Timestamp: 20:48:48:257_1
- RFN: 2030
- Chip: 18688
- Event: Cancel Timer
- Source: RRC_Def1 LINE 15
- Message Structure:
no details available
- Constraint:
t_T312
- BinaryMessage:

- No.: 1505
- Timestamp: 20:48:48:258_0
- RFN: 2030
- Chip: 20480
- Event: Default
- Source: RRC_Def1 LINE 0
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1506
- Timestamp: 20:48:48:258_1
- RFN: 2030
- Chip: 21504
- Event: Default
- Source: ts_RRC_Delay LINE 2
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1511
- Timestamp: 20:48:53:245_0
- RFN: 2529
- Chip: 10496
- Event: Timeout
- Source: ts_RRC_Delay LINE 2
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 1524
- Timestamp: 20:48:53:257_0
- RFN: 2530
- Chip: 17664
- Event: Send
- PCO: CMAC
- Message: CMAC_PAGING_Config_REQ
- Source: ts_CMAC_Pag1_Cfg LINE 4
- Message Structure:
CMAC_PAGING_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 5
. (RatType)ratType = 0
. CmacPagingConfigReq
. . pI_BitMapInfo
. . . (BitStringType)e18[18] = '010000000000000000'B
. . (IntegerType)dRX_CycleLength = 7
. . IMSI_GSM_MAP
. . . (IntegerType)_elem = 0
. . . (IntegerType)_elem = 0
. . . (IntegerType)_elem = 1
. . . (IntegerType)_elem = 0
. . . (IntegerType)_elem = 1
. . . (IntegerType)_elem = 0
. . . (IntegerType)_elem = 1
. . . (IntegerType)_elem = 2
. . . (IntegerType)_elem = 3
. . . (IntegerType)_elem = 4
. . . (IntegerType)_elem = 5
. . . (IntegerType)_elem = 6
. . . (IntegerType)_elem = 0
. . . (IntegerType)_elem = 6
. . . (IntegerType)_elem = 3
. . (BooleanType)t_pich_T_sccpch = FALSE
- Constraint:
ca_CMAC_PagingCfgReq
- BinaryMessage:
30 46 02 01 00 02 01 05 0a 01 00 30 3b 03 04 06 40 00 00 02 01 07 30 2d 02 01 00 02 01 00 02 01 01 02 01 00 02 01 01 02 01 00 02 01 01 02 01 02 02 01 03 02 01 04 02 01 05 02 01 06 02 01 00 02 01 06 02 01 03 01 01 00

- No.: 1525
- Timestamp: 20:48:53:261_0
- RFN: 2530
- Chip: 34560
- Event: Receive
- PCO: CMAC
- Message: CMAC_PAGING_Config_CNF
- Source: ts_CMAC_Pag1_Cfg LINE 5
- Message Structure:
CMAC_PAGING_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 5
- Constraint:
ca_CMAC_PagingCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 05

- No.: 1527
- Timestamp: 20:48:53:269_0
- RFN: 2531
- Chip: 27648
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_RRC_ConnEst_DCH_MT_PTMSI LINE 5
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -2
. tM_message
. . PCCH_Message
. . . PCCH_MessageType
. . . . PagingType1
. . . . . PagingRecordList
. . . . . . PagingRecord
. . . . . . . cn_Identity
. . . . . . . . (PagingCause)pagingCause = 2
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = 1
. . . . . . . . CN_PagedUE_Identity
. . . . . . . . . (BitStringType)p_TMSI_GSM_MAP[32] = "00010010001101000101011001111000"
. . . . . BCCH_ModificationInfo
. . . . . laterNonCriticalExtensions
- Constraint:
cas_PagingType1
- BinaryMessage:
30 0c 02 01 00 02 01 fe 40 54 24 68 ac f0

- No.: 1531
- Timestamp: 20:48:54:462_0
- RFN: 2650
- Chip: 36096
- Event: Receive
- PCO: TM
- Message: RLC_TR_DATA_IND
- Source: ts_RRC_ConnEst_DCH_MT_PTMSI LINE 6
- Message Structure:
RLC_TR_DATA_IND
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
. tM_message
. . UL_CCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode = 0
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . UL_CCCH_MessageType
. . . . RRCConnectionRequest
. . . . . InitialUE_Identity
. . . . . . TMSI_and_LAI_GSM_MAP
. . . . . . . (BitStringType)tmsi[32] = "00010010001101000101011001111000"
. . . . . . . LAI
. . . . . . . . PLMN_Identity
. . . . . . . . . MCC
. . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . (IntegerType)_elem = 1
. . . . . . . . . MNC
. . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . (IntegerType)_elem = 1
. . . . . . . . (BitStringType)lac[16] = '0000000000000001'B
. . . . . (EstablishmentCause)establishmentCause = 7
. . . . . (ProtocolErrorIndicator)protocolErrorIndicator = 0
. . . . . MeasuredResultsOnRACH
. . . . . . currentCell
. . . . . . . modeSpecificInfo
. . . . . . . . fdd
. . . . . . . . . measurementQuantity
. . . . . . . . . . (IntegerType)cpich_Ec_N0 = 0
. . . . . v3d0NonCriticalExtensions
. . . . . . RRCConnectionRequest_v3d0ext_IEs
. . . . . . . (BitStringType)uESpecificBehaviourInformation1idle = 0
. . . . . . nonCriticalExtensions
- Constraint:
car_RRC_ConnReq
- BinaryMessage:
30 11 02 01 00 02 01 00 21 12 34 56 78 00 10 08 00 09 c0

- No.: 1532
- Timestamp: 20:48:54:526_0
- RFN: 2657
- Chip: 13824
- Event: Send
- PCO: UM
- Message: RLC_UM_DATA_REQ
- Source: ts_RRC_ConnEst_DCH_MT_PTMSI LINE 7
- Message Structure:
RLC_UM_DATA_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
. uM_message
. . DL_CCCH_Message
. . . IntegrityCheckInfo
. . . DL_CCCH_MessageType
. . . . RRCConnectionSetup
. . . . . r3
. . . . . . RRCConnectionSetup_r3_IEs
. . . . . . . InitialUE_Identity
. . . . . . . . TMSI_and_LAI_GSM_MAP
. . . . . . . . . (BitStringType)tmsi[32] = "00010010001101000101011001111000"
. . . . . . . . . LAI
. . . . . . . . . . PLMN_Identity
. . . . . . . . . . . MCC
. . . . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . . . (IntegerType)_elem = 1
. . . . . . . . . . . MNC
. . . . . . . . . . . . (IntegerType)_elem = 0
. . . . . . . . . . . . (IntegerType)_elem = 1
. . . . . . . . . . (BitStringType)lac[16] = '0000000000000001'B
. . . . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . . . (IntegerType)activationTime = -
. . . . . . . U_RNTI
. . . . . . . . (BitStringType)srnc_Identity[12] = "000000000001"
. . . . . . . . (BitStringType)s_RNTI[20] = "00000000000000000001"
. . . . . . . (BitStringType)new_c_RNTI[16] = -
. . . . . . . (RRC_StateIndicator)rrc_StateIndicator = 0
. . . . . . . (IntegerType)utran_DRX_CycleLengthCoeff = 9
. . . . . . . CapabilityUpdateRequirement
. . . . . . . . (BooleanType)ue_RadioCapabilityFDDUpdateRequirement = TRUE
. . . . . . . . (BooleanType)ue_RadioCapabilityTDDUpdateRequirement = FALSE
. . . . . . . . SystemSpecificCapUpdateReqList
. . . . . . . . . (SystemSpecificCapUpdateReq)_elem = 0
. . . . . . . SRB_InformationSetupList2
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_UM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 1
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 1
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . . . . . . . (TimerRST)timerRST = 9
. . . . . . . . . . . . . (MaxRST)max_RST = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 2
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 2
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . . . . . . . (TimerRST)timerRST = 9
. . . . . . . . . . . . . (MaxRST)max_RST = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 3
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 3
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity = -
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize = 3
. . . . . . . . . . . . . (TimerRST)timerRST = 9
. . . . . . . . . . . . . (MaxRST)max_RST = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll = 39
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 4
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 4
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . UL_CommonTransChInfo
. . . . . . . . TFC_Subset
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . TFCS
. . . . . . . . . . . ExplicitTFCS_Configuration
. . . . . . . . . . . . TFCS_ReconfAdd
. . . . . . . . . . . . . ctfcSize
. . . . . . . . . . . . . . ctfc2Bit
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . . . . . . . (IntegerType)ctfc2 = 0
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . . . . . . . (IntegerType)ctfc2 = 1
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 11
. . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . UL_AddReconfTransChInfoList
. . . . . . . . UL_AddReconfTransChInformation
. . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType = 0
. . . . . . . . . (IntegerType)transportChannelIdentity = 5
. . . . . . . . . TransportFormatSet
. . . . . . . . . . DedicatedTransChTFS
. . . . . . . . . . . tti
. . . . . . . . . . . . DedicatedDynamicTF_InfoList
. . . . . . . . . . . . . DedicatedDynamicTF_Info
. . . . . . . . . . . . . . rlc_Size
. . . . . . . . . . . . . . . BitModeRLC_SizeInfo
. . . . . . . . . . . . . . . . sizeType2
. . . . . . . . . . . . . . . . . (IntegerType)part1 = 2
. . . . . . . . . . . . . . . . . (IntegerType)part2 = -
. . . . . . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . LogicalChannelList
. . . . . . . . . . . SemistaticTF_Information
. . . . . . . . . . . . ChannelCodingType
. . . . . . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . . . . . (IntegerType)rateMatchingAttribute = 192
. . . . . . . . . . . . (CRC_Size)crc_Size = 3
. . . . . . . DL_CommonTransChInfo
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . dl_Parameters
. . . . . . . DL_AddReconfTransChInfoList
. . . . . . . . DL_AddReconfTransChInformation
. . . . . . . . . (DL_TrCH_Type)dl_TransportChannelType = 0
. . . . . . . . . (IntegerType)dl_transportChannelIdentity = 10
. . . . . . . . . tfs_SignallingMode
. . . . . . . . . . UL_TransportChannelIdentity
. . . . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType = 0
. . . . . . . . . . . (IntegerType)ul_TransportChannelIdentity = 5
. . . . . . . . . QualityTarget
. . . . . . . . . . (IntegerType)bler_QualityValue = -20
. . . . . . . . . TM_SignallingInfo
. . . . . . . FrequencyInfo
. . . . . . . (IntegerType)maxAllowedUL_TX_Power = -
. . . . . . . UL_ChannelRequirement
. . . . . . . . UL_DPCH_Info
. . . . . . . . . UL_DPCH_PowerControlInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (IntegerType)dpcch_PowerOffset = -40
. . . . . . . . . . . (IntegerType)pc_Preamble = 1
. . . . . . . . . . . (IntegerType)sRB_delay = 7
. . . . . . . . . . . PowerControlAlgorithm
. . . . . . . . . . . . (IntegerType)algorithm1 = 1
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (ScramblingCodeType)scramblingCodeType = 1
. . . . . . . . . . . (IntegerType)scramblingCode = 0
. . . . . . . . . . . (IntegerType)numberOfDPDCH = -
. . . . . . . . . . . (SpreadingFactor)spreadingFactor = 4
. . . . . . . . . . . (BooleanType)tfci_Existence = TRUE
. . . . . . . . . . . (IntegerType)numberOfFBI_Bits = -
. . . . . . . . . . . (PuncturingLimit)puncturingLimit = 15
. . . . . . . DL_CommonInformation
. . . . . . . . DL_DPCH_InfoCommon
. . . . . . . . . cfnHandling
. . . . . . . . . . initialise
. . . . . . . . . . . (IntegerType)cfntargetsfnframeoffset = -
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . DL_DPCH_PowerControlInfo
. . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . (DPC_Mode)dpc_Mode = 0
. . . . . . . . . . . (IntegerType)powerOffsetPilot_pdpdch = 0
. . . . . . . . . . . Dl_rate_matching_restriction
. . . . . . . . . . . SF512_AndPilot
. . . . . . . . . . . . (PilotBits128)sfd128 = 0
. . . . . . . . . . . (PositionFixedOrFlexible)positionFixedOrFlexible = 0
. . . . . . . . . . . (BooleanType)tfci_Existence = FALSE
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . (IntegerType)defaultDPCH_OffsetValue = 0
. . . . . . . . . . DPCH_CompressedModeInfo
. . . . . . . . . . (TX_DiversityMode)tx_DiversityMode = 0
. . . . . . . . . . SSDT_Information
. . . . . . . DL_InformationPerRL_List
. . . . . . . . DL_InformationPerRL
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . PrimaryCPICH_Info
. . . . . . . . . . . . (IntegerType)primaryScramblingCode = 100
. . . . . . . . . . . PDSCH_SHO_DCH_Info
. . . . . . . . . . . PDSCH_CodeMapping
. . . . . . . . . DL_DPCH_InfoPerRL
. . . . . . . . . . fdd
. . . . . . . . . . . (PCPICH_UsageForChannelEst)pCPICH_UsageForChannelEst = 0
. . . . . . . . . . . (IntegerType)dpch_FrameOffset = 0
. . . . . . . . . . . SecondaryCPICH_Info
. . . . . . . . . . . DL_ChannelisationCodeList
. . . . . . . . . . . . DL_ChannelisationCode
. . . . . . . . . . . . . (IntegerType)secondaryScramblingCode = 1
. . . . . . . . . . . . . SF512_AndCodeNumber
. . . . . . . . . . . . . . (IntegerType)sf128 = 0
. . . . . . . . . . . . . (ScramblingCodeChange)scramblingCodeChange = 1
. . . . . . . . . . . (IntegerType)tpc_CombinationIndex = 0
. . . . . . . . . . . (SSDT_CellIdentity)ssdt_CellIdentity = -
. . . . . . . . . . . (ClosedLoopTimingAdjMode)closedLoopTimingAdjMode = -
. . . . . . . . . SCCPCH_InfoForFACH
. . . . . . laterNonCriticalExtensions
. (BooleanType)specialLI = TRUE
- Constraint:
cas_RRC_ConnSetup
- BinaryMessage:
30 78 02 01 00 02 01 00 30 e7 22 46 8a cf 00 02 01 00 01 00 04 00 00 4d 82 69 3a 10 10 89 0d 42 00 02 81 9e 8e 46 c9 ce 7c 9c 4e 74 20 a5 12 3a 8c 00 15 13 3d 1c 8d 93 9c f9 38 9c e8 42 52 24 b5 28 00 4a 46 7a 39 1b 27 39 f2 71 39 d0 86 b4 49 ea 70 00 d4 c8 00 06 25 2b f0 02 00 08 82 23 bf 66 08 98 95 a5 47 a2 00 00 01 3f 90 0a 14 00 02 06 40 00 0c 28 08 01 01 ff

- No.: 1540
- Timestamp: 20:48:54:567_2
- RFN: 2661
- Chip: 15616
- Event: Start Timer
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 3
- Message Structure:
no details available
- Constraint:
t_WaitMS (13500 Ms)
- BinaryMessage:

- No.: 1545
- Timestamp: 20:48:54:790_0
- RFN: 2683
- Chip: 30976
- Event: Receive
- PCO: CPHY
- Message: CPHY_Sync_IND
- Source: RRC_Def1 LINE 13
- Message Structure:
CPHY_Sync_IND
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_SyncInd
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 1546
- Timestamp: 20:48:54:791_0
- RFN: 2683
- Chip: 32768
- Event: Cancel Timer
- Source: RRC_Def1 LINE 13
- Message Structure:
no details available
- Constraint:
t_T312
- BinaryMessage:

- No.: 1547
- Timestamp: 20:48:54:791_1
- RFN: 2683
- Chip: 34560
- Event: Default
- Source: RRC_Def1 LINE 0
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1548
- Timestamp: 20:48:54:792_0
- RFN: 2683
- Chip: 35328
- Event: Default
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1553
- Timestamp: 20:48:54:906_0
- RFN: 2695
- Chip: 11264
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_IND
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
RLC_AM_DATA_IND
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. IntegrityResult
. . (IntegrityStatus)integrityUsed = 0
. aM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode = 0
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . UL_DCCH_MessageType
. . . . RRCConnectionSetupComplete
. . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . STARTList
. . . . . . STARTSingle
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity = 1
. . . . . . . (BitStringType)start_Value[20] = "00000000000000000010"
. . . . . . STARTSingle
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity = 0
. . . . . . . (BitStringType)start_Value[20] = "00000000000000000010"
. . . . . UE_RadioAccessCapability
. . . . . . (AccessStratumReleaseIndicator)accessStratumReleaseIndicator = 0
. . . . . . PDCP_Capability
. . . . . . . (BooleanType)losslessSRNS_RelocationSupport = FALSE
. . . . . . . supportForRfc2507
. . . . . . RLC_Capability
. . . . . . . (TotalRLC_AM_BufferSize)totalRLC_AM_BufferSize = 2
. . . . . . . (MaximumRLC_WindowSize)maximumRLC_WindowSize = 0
. . . . . . . (MaximumAM_EntityNumberRLC_Cap)maximumAM_EntityNumber = 3
. . . . . . TransportChannelCapability
. . . . . . . DL_TransChCapability
. . . . . . . . (MaxNoBits)maxNoBitsReceived = 4
. . . . . . . . (MaxNoBits)maxConvCodeBitsReceived = 1
. . . . . . . . TurboSupport
. . . . . . . . . (MaxNoBits)supported = 4
. . . . . . . . (MaxSimultaneousTransChsDL)maxSimultaneousTransChs = 1
. . . . . . . . (IntegerType)maxSimultaneousCCTrCH_Count = 1
. . . . . . . . (MaxTransportBlocksDL)maxReceivedTransportBlocks = 2
. . . . . . . . (MaxNumberOfTFC_DL)maxNumberOfTFC = 4
. . . . . . . . (MaxNumberOfTF)maxNumberOfTF = 1
. . . . . . . UL_TransChCapability
. . . . . . . . (MaxNoBits)maxNoBitsTransmitted = 3
. . . . . . . . (MaxNoBits)maxConvCodeBitsTransmitted = 1
. . . . . . . . TurboSupport
. . . . . . . . . (MaxNoBits)supported = 3
. . . . . . . . (MaxSimultaneousTransChsUL)maxSimultaneousTransChs = 2
. . . . . . . . modeSpecificInfo
. . . . . . . . (MaxTransportBlocksUL)maxTransmittedBlocks = 2
. . . . . . . . (MaxNumberOfTFC_UL)maxNumberOfTFC = 3
. . . . . . . . (MaxNumberOfTF)maxNumberOfTF = 0
. . . . . . RF_Capability
. . . . . . . fddRF_Capability
. . . . . . . . (IntegerType)ue_PowerClass = 4
. . . . . . . . (TxRxFrequencySeparation)txRxFrequencySeparation = 0
. . . . . . . tddRF_Capability
. . . . . . . . (IntegerType)ue_PowerClass = 0
. . . . . . . . (RadioFrequencyBandTDDList)radioFrequencyTDDBandList = 0
. . . . . . . . (ChipRateCapability)chipRateCapability = 0
. . . . . . PhysicalChannelCapability
. . . . . . . fddPhysChCapability
. . . . . . . . DL_PhysChCapabilityFDD
. . . . . . . . . (IntegerType)maxNoDPCH_PDSCH_Codes = 3
. . . . . . . . . (MaxNoPhysChBitsReceived)maxNoPhysChBitsReceived = 6
. . . . . . . . . (BooleanType)supportForSF_512 = FALSE
. . . . . . . . . (BooleanType)supportOfPDSCH = FALSE
. . . . . . . . . SimultaneousSCCPCH_DPCH_Reception
. . . . . . . . UL_PhysChCapabilityFDD
. . . . . . . . . (MaxNoDPDCH_BitsTransmitted)maxNoDPDCH_BitsTransmitted = 2
. . . . . . . . . (BooleanType)supportOfPCPCH = FALSE
. . . . . . . tddPhysChCapability
. . . . . . . . DL_PhysChCapabilityTDD
. . . . . . . . . (IntegerType)maxTS_PerFrame = 0
. . . . . . . . . (IntegerType)maxPhysChPerFrame = 0
. . . . . . . . . (MinimumSF_DL)minimumSF = 0
. . . . . . . . . (BooleanType)supportOfPDSCH = FALSE
. . . . . . . . . (IntegerType)maxPhysChPerTS = 0
. . . . . . . . UL_PhysChCapabilityTDD
. . . . . . . . . (IntegerType)maxTS_PerFrame = 0
. . . . . . . . . (MaxPhysChPerTimeslot)maxPhysChPerTimeslot = 0
. . . . . . . . . (MinimumSF_UL)minimumSF = 0
. . . . . . . . . (BooleanType)supportOfPUSCH = FALSE
. . . . . . UE_MultiModeRAT_Capability
. . . . . . . MultiRAT_Capability
. . . . . . . . (BooleanType)supportOfGSM = TRUE
. . . . . . . . (BooleanType)supportOfMulticarrier = FALSE
. . . . . . . (MultiModeCapability)multiModeCapability = 1
. . . . . . SecurityCapability
. . . . . . . (BitStringType)cipheringAlgorithmCap[16] = '0000000000000011'B
. . . . . . . (BitStringType)integrityProtectionAlgorithmCap[16] = '0000000000000010'B
. . . . . . UE_Positioning_Capability
. . . . . . . (BooleanType)standaloneLocMethodsSupported = FALSE
. . . . . . . (BooleanType)ue_BasedOTDOA_Supported = FALSE
. . . . . . . (NetworkAssistedGPS_Supported)networkAssistedGPS_Supported = 3
. . . . . . . (BooleanType)supportForUE_GPS_TimingOfCellFrames = FALSE
. . . . . . . (BooleanType)supportForIPDL = FALSE
. . . . . . MeasurementCapability
. . . . . . . CompressedModeMeasCapability
. . . . . . . . (BooleanType)fdd_Measurements = TRUE
. . . . . . . . (BooleanType)tdd_Measurements = FALSE
. . . . . . . . GSM_Measurements
. . . . . . . . . (BooleanType)gsm900 = TRUE
. . . . . . . . . (BooleanType)dcs1800 = TRUE
. . . . . . . . . (BooleanType)gsm1900 = FALSE
. . . . . . . . (BooleanType)multiCarrierMeasurements = FALSE
. . . . . . . CompressedModeMeasCapability
. . . . . . . . (BooleanType)fdd_Measurements = TRUE
. . . . . . . . (BooleanType)tdd_Measurements = FALSE
. . . . . . . . GSM_Measurements
. . . . . . . . . (BooleanType)gsm900 = TRUE
. . . . . . . . . (BooleanType)dcs1800 = TRUE
. . . . . . . . . (BooleanType)gsm1900 = FALSE
. . . . . . . . (BooleanType)multiCarrierMeasurements = FALSE
. . . . . v370NonCriticalExtensions
. . . . . . RRCConnectionSetupComplete_v370ext
. . . . . . . UE_RadioAccessCapability_v370ext
. . . . . . v380NonCriticalExtensions
. . . . . . . RRCConnectionSetupComplete_v380ext_IEs
. . . . . . . . UE_RadioAccessCapability_v380ext
. . . . . . . . . UE_PositioningCapabilityExt_v380
. . . . . . . . . . (BooleanType)rx_tx_TimeDifferenceType2Capable = FALSE
. . . . . . . . DL_PhysChCapabilityFDD_v380ext
. . . . . . . . . (SupportOfDedicatedPilotsForChEstimation)supportOfDedicatedPilotsForChEstimation = 0
. . . . . . . v3a0NonCriticalExtensions
. . . . . . . . RRCConnectionSetupComplete_v3a0ext_IEs
. . . . . . . . . UE_RadioAccessCapability_v3a0ext
. . . . . . . . . . UE_PositioningCapabilityExt_v3a0
. . . . . . . . . . . (UE_PositioningCapabilityExt_v3a0_list_0)validity_CellPCH_UraPCH = 0
. . . . . . . . laterNonCriticalExtensions
. . . . . . . . . (BitStringType)rrcConnectionSetupComplete_r3_add_ext = 0
. . . . . . . . . nonCriticalExtensions
- Constraint:
car_RRC_ConnSetupCmpl
- BinaryMessage:
30 27 02 01 ff 02 01 02 0a 05 01 00 00 00 00 4a 0c 00 00 80 00 05 11 a0 d1 04 84 c6 68 46 2c 93 02 48 00 18 00 11 8f 8f 80

- No.: 1554
- Timestamp: 20:48:54:916_0
- RFN: 2696
- Chip: 12544
- Event: Cancel Timer
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
t_WaitMS
- BinaryMessage:

- No.: 1555
- Timestamp: 20:48:54:917_0
- RFN: 2696
- Chip: 13568
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 5
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1569
- Timestamp: 20:48:54:923_0
- RFN: 2697
- Chip: 0
- Event: Send
- PCO: CMAC
- Message: CMAC_SecurityMode_Config_REQ
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 1
- Message Structure:
CMAC_SecurityMode_Config_REQ
. (IntegerType)cellId = 0
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity = 1
. . (BitStringType)startValue[20] = "00000000000000000010"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = -
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CMAC_SecurityModeCfgReq
- BinaryMessage:
30 0e 02 01 00 30 09 0a 01 01 03 04 04 00 00 20

- No.: 1570
- Timestamp: 20:48:54:925_0
- RFN: 2697
- Chip: 6656
- Event: Receive
- PCO: CMAC
- Message: CMAC_SecurityMode_Config_CNF
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 2
- Message Structure:
CMAC_SecurityMode_Config_CNF
. (IntegerType)cellId = 0
- Constraint:
ca_CMAC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 00

- No.: 1571
- Timestamp: 20:48:54:927_0
- RFN: 2697
- Chip: 13824
- Event: Send
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_REQ
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 3
- Message Structure:
CRLC_SecurityMode_Config_REQ
. (IntegerType)cellId = -1
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity = 1
. . (BitStringType)startValue[20] = "00000000000000000010"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = -
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CRLC_SecurityModeCfgReq
- BinaryMessage:
30 0e 02 01 ff 30 09 0a 01 01 03 04 04 00 00 20

- No.: 1572
- Timestamp: 20:48:54:928_0
- RFN: 2697
- Chip: 20480
- Event: Receive
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_CNF
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 4
- Message Structure:
CRLC_SecurityMode_Config_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1586
- Timestamp: 20:48:54:934_0
- RFN: 2698
- Chip: 3072
- Event: Send
- PCO: CMAC
- Message: CMAC_SecurityMode_Config_REQ
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 1
- Message Structure:
CMAC_SecurityMode_Config_REQ
. (IntegerType)cellId = 0
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity = 0
. . (BitStringType)startValue[20] = "00000000000000000010"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = -
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CMAC_SecurityModeCfgReq
- BinaryMessage:
30 0e 02 01 00 30 09 0a 01 00 03 04 04 00 00 20

- No.: 1587
- Timestamp: 20:48:54:935_0
- RFN: 2698
- Chip: 9216
- Event: Receive
- PCO: CMAC
- Message: CMAC_SecurityMode_Config_CNF
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 2
- Message Structure:
CMAC_SecurityMode_Config_CNF
. (IntegerType)cellId = 0
- Constraint:
ca_CMAC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 00

- No.: 1588
- Timestamp: 20:48:54:937_0
- RFN: 2698
- Chip: 16384
- Event: Send
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_REQ
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 3
- Message Structure:
CRLC_SecurityMode_Config_REQ
. (IntegerType)cellId = -1
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity = 0
. . (BitStringType)startValue[20] = "00000000000000000010"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = -
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CRLC_SecurityModeCfgReq
- BinaryMessage:
30 0e 02 01 ff 30 09 0a 01 00 03 04 04 00 00 20

- No.: 1589
- Timestamp: 20:48:54:939_0
- RFN: 2698
- Chip: 23296
- Event: Receive
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_CNF
- Source: ts_SS_SecurityDownloadStartCN_Domain:lt_DownloadKey LINE 4
- Message Structure:
CRLC_SecurityMode_Config_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1610
- Timestamp: 20:48:54:949_0
- RFN: 2699
- Chip: 24320
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: pr_GenericSetupProcedures:lt_ReceiveResponseToPaging LINE 2
- Message Structure:
RRC_DataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. (START_Value)start[20] = '00000000000000000010'B
. SERVICEREQUEST
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)gMMProtocolDiscriminator[4] = '1000'B
. . (MsgType)msgType[8] = '00001100'B
. . ServiceType_v
. . . (B1)spare1[1] = '0'B
. . . (B3)type[3] = '010'B
. . CiphKeySeqNum
. . . (B1)spare1[1] = '0'B
. . . (KeySeq)keySeq[3] = '000'B
. . MS_Identity_lv
. . . (Length)iel[1] = '05'O
. . . (B4)iDigit1[4] = '1111'B
. . . (B1)oddEvenInd[1] = '0'B
. . . (B3)typeOfId[3] = '100'B
. . . (OctetStringType)otherDigits[4] = '12345678'O
. . PDP_ContextStatus
. . . (IEI8)iei[8] = '00110010'B
. . . (Length)iel[1] = '02'O
. . . (BitStringType)nSAPI[16] = '0000000000000000'B
- Constraint:
car_PS_InitDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 03 04 04 00 00 20 08 0c 20 05 f4 12 34 56 78 32 02 00 00

- No.: 1644
- Timestamp: 20:48:54:963_0
- RFN: 2701
- Chip: 256
- Event: Send
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_REQ
- Source: ts_SS_DownloadSecurityKey:lt_DownloadKeyCRLC LINE 1
- Message Structure:
CRLC_SecurityMode_Config_REQ
. (IntegerType)cellId = -1
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity = 1
. . (BitStringType)startValue[20] = "00000000000000000010"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = '01010111010101100101000101010000010100110101001001011101010111000101111101011110010110010101100001011011010110100101010101010100'B
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CRLC_SecurityModeCfgReq
- BinaryMessage:
30 21 02 01 ff 30 1c 0a 01 01 03 04 04 00 00 20 03 11 00 57 56 51 50 53 52 5d 5c 5f 5e 59 58 5b 5a 55 54

- No.: 1645
- Timestamp: 20:48:54:965_0
- RFN: 2701
- Chip: 7424
- Event: Receive
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_CNF
- Source: ts_SS_DownloadSecurityKey:lt_DownloadKeyCRLC LINE 2
- Message Structure:
CRLC_SecurityMode_Config_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1652
- Timestamp: 20:48:54:968_0
- RFN: 2701
- Chip: 19968
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 1
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
. (IntegerType)count_I_LSB_UL = -
. (IntegerType)count_I_LSB_DL = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 00 02 01 00 02 01 00

- No.: 1653
- Timestamp: 20:48:54:970_0
- RFN: 2701
- Chip: 27648
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 2
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 00 02 01 00

- No.: 1654
- Timestamp: 20:48:54:972_0
- RFN: 2701
- Chip: 35840
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 3
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. (IntegerType)count_I_LSB_UL = -
. (IntegerType)count_I_LSB_DL = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 01 02 01 00

- No.: 1655
- Timestamp: 20:48:54:974_0
- RFN: 2702
- Chip: 4864
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 4
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 1656
- Timestamp: 20:48:54:976_0
- RFN: 2702
- Chip: 12032
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 5
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. (IntegerType)count_I_LSB_UL = -
. (IntegerType)count_I_LSB_DL = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 02 02 01 00

- No.: 1657
- Timestamp: 20:48:54:978_0
- RFN: 2702
- Chip: 19200
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 6
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 1658
- Timestamp: 20:48:54:980_0
- RFN: 2702
- Chip: 26112
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 7
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
. (IntegerType)count_I_LSB_UL = -
. (IntegerType)count_I_LSB_DL = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 03 02 01 00

- No.: 1659
- Timestamp: 20:48:54:982_0
- RFN: 2702
- Chip: 33792
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 8
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 1660
- Timestamp: 20:48:54:983_0
- RFN: 2703
- Chip: 2304
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 9
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
. (IntegerType)count_I_LSB_UL = -
. (IntegerType)count_I_LSB_DL = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 04 02 01 00

- No.: 1661
- Timestamp: 20:48:54:985_0
- RFN: 2703
- Chip: 9216
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 10
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 1665
- Timestamp: 20:48:54:988_0
- RFN: 2703
- Chip: 20480
- Event: Send
- PCO: CRLC
- Message: CRLC_Integrity_Activate_REQ
- Source: ts_CRLC_DL_Integrity LINE 1
- Message Structure:
CRLC_Integrity_Activate_REQ
. (IntegerType)cellId = -1
. (CN_DomainIdentity)cn_DomainIdentity = 1
. IntegrityActivationInfo
. . IntegrityProtectionModeInfo
. . . IntegrityProtectionModeCommand
. . . . startIntegrityProtection
. . . . . (BitStringType)integrityProtInitNumber[32] = "00000000000000000000000000000001"
. . . (IntegrityProtectionAlgorithm)integrityProtectionAlgorithm = 0
- Constraint:
ca_CRLC_DL_IntegrityActivateReq
- BinaryMessage:
30 15 02 01 ff 0a 01 01 30 0d 30 30 07 03 05 00 00 00 00 01 0a 01 00

- No.: 1666
- Timestamp: 20:48:54:990_0
- RFN: 2703
- Chip: 26624
- Event: Receive
- PCO: CRLC
- Message: CRLC_Integrity_Activate_CNF
- Source: ts_CRLC_DL_Integrity LINE 2
- Message Structure:
CRLC_Integrity_Activate_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_IntegrityActivateCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1673
- Timestamp: 20:48:54:994_0
- RFN: 2704
- Chip: 3072
- Event: Send
- PCO: CRLC
- Message: CRLC_Integrity_Activate_REQ
- Source: ts_RB2_UL_IntegrityActivate LINE 1
- Message Structure:
CRLC_Integrity_Activate_REQ
. (IntegerType)cellId = -1
. (CN_DomainIdentity)cn_DomainIdentity = 1
. IntegrityActivationInfo
. . IntegrityProtActivationInfoList
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity = 2
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
- Constraint:
ca_CRLC_UL_IntegrityActivateReq
- BinaryMessage:
30 10 02 01 ff 0a 01 01 30 08 30 06 02 01 02 02 01 00

- No.: 1674
- Timestamp: 20:48:54:995_0
- RFN: 2704
- Chip: 8960
- Event: Receive
- PCO: CRLC
- Message: CRLC_Integrity_Activate_CNF
- Source: ts_RB2_UL_IntegrityActivate LINE 2
- Message Structure:
CRLC_Integrity_Activate_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_IntegrityActivateCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1680
- Timestamp: 20:48:55:001_0
- RFN: 2704
- Chip: 33024
- Event: Send
- PCO: AM
- Message: RLC_AM_DATA_REQ
- Source: ts_RRC_Security:lt_SendSecurityModeCommand LINE 7
- Message Structure:
RLC_AM_DATA_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. AmConfirmationRequest
. aM_message
. . DL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00000000000000000000000000000000"
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . DL_DCCH_MessageType
. . . . SecurityModeCommand
. . . . . r3
. . . . . . SecurityModeCommand_r3_IEs
. . . . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . . . SecurityCapability
. . . . . . . . (BitStringType)cipheringAlgorithmCap[16] = '0000000000000011'B
. . . . . . . . (BitStringType)integrityProtectionAlgorithmCap[16] = '0000000000000010'B
. . . . . . . CipheringModeInfo
. . . . . . . IntegrityProtectionModeInfo
. . . . . . . . IntegrityProtectionModeCommand
. . . . . . . . . startIntegrityProtection
. . . . . . . . . . (BitStringType)integrityProtInitNumber[32] = "00000000000000000000000000000001"
. . . . . . . . (IntegrityProtectionAlgorithm)integrityProtectionAlgorithm = 0
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity = 1
. . . . . . . InterRAT_UE_SecurityCapList
. . . . . . laterNonCriticalExtensions
- Constraint:
cas_RRC_SecModeCmd
- BinaryMessage:
30 17 02 01 ff 02 01 02 05 00 80 00 00 00 04 04 00 01 80 01 40 00 00 00 30

- No.: 1686
- Timestamp: 20:48:55:135_0
- RFN: 2718
- Chip: 12288
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_IND
- Source: ts_RRC_Security:lt_StartSecurity_UE LINE 8
- Message Structure:
RLC_AM_DATA_IND
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. IntegrityResult
. . (IntegrityStatus)integrityUsed = 0
. aM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "11101101011010000100111100101101"
. . . . (IntegerType)rrc_MessageSequenceNumber = 1
. . . UL_DCCH_MessageType
. . . . SecurityModeComplete
. . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . IntegrityProtActivationInfo
. . . . . . RRC_MessageSequenceNumberList
. . . . . . . (IntegerType)_elem = 0
. . . . . . . (IntegerType)_elem = 0
. . . . . . . (IntegerType)_elem = 0
. . . . . . . (IntegerType)_elem = 0
. . . . . . . (IntegerType)_elem = 0
. . . . . laterNonCriticalExtensions
. . . . . . (BitStringType)securityModeComplete_r3_add_ext = 0
. . . . . . nonCriticalExtensions
- Constraint:
car_RRC_SecModeCmpl
- BinaryMessage:
30 12 02 01 ff 02 01 02 0a 01 00 f6 b4 27 96 8d 21 00 00 00

- No.: 1687
- Timestamp: 20:48:55:137_0
- RFN: 2718
- Chip: 16384
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_Security:lt_StartSecurity_UE LINE 8
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1689
- Timestamp: 20:48:55:141_0
- RFN: 2718
- Chip: 33536
- Event: Send
- PCO: CRLC
- Message: CRLC_Integrity_Activate_REQ
- Source: ts_CRLC_UL_Integrity LINE 1
- Message Structure:
CRLC_Integrity_Activate_REQ
. (IntegerType)cellId = -1
. (CN_DomainIdentity)cn_DomainIdentity = 1
. IntegrityActivationInfo
. . IntegrityProtActivationInfoList
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity = 0
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity = 1
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity = 3
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity = 4
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
- Constraint:
ca_CRLC_UL_IntegrityActivateReq
- BinaryMessage:
30 28 02 01 ff 0a 01 01 30 20 30 06 02 01 00 02 01 00 30 06 02 01 01 02 01 00 30 06 02 01 03 02 01 00 30 06 02 01 04 02 01 00

- No.: 1690
- Timestamp: 20:48:55:143_0
- RFN: 2719
- Chip: 2304
- Event: Receive
- PCO: CRLC
- Message: CRLC_Integrity_Activate_CNF
- Source: ts_CRLC_UL_Integrity LINE 2
- Message Structure:
CRLC_Integrity_Activate_CNF
. (IntegerType)cellId = -1
- Constraint:
ca_CRLC_IntegrityActivateCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1702
- Timestamp: 20:48:55:148_0
- RFN: 2719
- Chip: 22272
- Event: Send
- PCO: Dc
- Message: RRC_DataReq
- Source: ts_TC_ActivateRB_TestMode LINE 7
- Message Structure:
RRC_DataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[-1] = -
. (SapId)sapId[1] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. ACTIVATERBTESTMODE
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)tCProtocolDiscriminator[4] = '1111'B
. . (MsgType)msgType[8] = '01000100'B
- Constraint:
ca_PS_DataReq
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 0f 44

- No.: 1703
- Timestamp: 20:48:55:149_0
- RFN: 2719
- Chip: 25856
- Event: Start Timer
- Source: ts_TC_ActivateRB_TestMode LINE 7
- Message Structure:
no details available
- Constraint:
t_Dly (5000 Ms)
- BinaryMessage:

- No.: 1707
- Timestamp: 20:48:55:274_0
- RFN: 2732
- Chip: 4352
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_TC_ActivateRB_TestMode LINE 8
- Message Structure:
RRC_DataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. (START_Value)start[0] = -
. ACTIVATERBTESTMODECOMPLETE
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)tCProtocolDiscriminator[4] = '1111'B
. . (MsgType)msgType[8] = '01000101'B
- Constraint:
car_PS_UplinkDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 0f 45

- No.: 1708
- Timestamp: 20:48:55:275_0
- RFN: 2732
- Chip: 7680
- Event: Cancel Timer
- Source: ts_TC_ActivateRB_TestMode LINE 8
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 1709
- Timestamp: 20:48:55:275_1
- RFN: 2732
- Chip: 8448
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_TC_ActivateRB_TestMode LINE 8
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1728
- Timestamp: 20:48:55:302_0
- RFN: 2734
- Chip: 37120
- Event: Send
- PCO: CPHY
- Message: CPHY_Frame_Number_REQ
- Source: ts_RRC_SetUpRAB_AM_7_RLC LINE 2
- Message Structure:
CPHY_Frame_Number_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
cas_GetFrameNum
- BinaryMessage:
30 06 02 01 00 02 01 1a

- No.: 1732
- Timestamp: 20:48:55:314_0
- RFN: 2736
- Chip: 6656
- Event: Receive
- PCO: CPHY
- Message: CPHY_Frame_Number_CNF
- Source: ts_RRC_SetUpRAB_AM_7_RLC LINE 3
- Message Structure:
CPHY_Frame_Number_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
. (IntegerType)frameNumber = 175
- Constraint:
car_GetFrameNum
- BinaryMessage:
30 0a 02 01 00 02 01 1a 02 02 00 af

- No.: 1736
- Timestamp: 20:48:55:361_0
- RFN: 2740
- Chip: 31744
- Event: Send
- PCO: AM
- Message: RLC_AM_DATA_REQ
- Source: ts_RRC_SetUpRAB_AM_7_RLC:lt_SendRAB_SetupCS_OrPS LINE 4
- Message Structure:
RLC_AM_DATA_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. AmConfirmationRequest
. . (IntegerType)confirmationRequested = 0
. aM_message
. . DL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00000000000000000000000000000000"
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . DL_DCCH_MessageType
. . . . RadioBearerSetup
. . . . . r3
. . . . . . RadioBearerSetup_r3_IEs
. . . . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . . . IntegrityProtectionModeInfo
. . . . . . . CipheringModeInfo
. . . . . . . (IntegerType)activationTime = 160
. . . . . . . U_RNTI
. . . . . . . (BitStringType)new_C_RNTI[16] = -
. . . . . . . (RRC_StateIndicator)rrc_StateIndicator = 0
. . . . . . . (IntegerType)utran_DRX_CycleLengthCoeff = -
. . . . . . . (BitStringType)ura_Identity[0] = -
. . . . . . . CN_InformationInfo
. . . . . . . SRB_InformationSetupList
. . . . . . . RAB_InformationSetupList
. . . . . . . . RAB_InformationSetup
. . . . . . . . . RAB_Info
. . . . . . . . . . RAB_Identity
. . . . . . . . . . . (BitStringType)gsm_MAP_RAB_Identity[8] = '00000101'B
. . . . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = 1
. . . . . . . . . . (BitStringType)nas_Synchronisation_Indicator[0] = -
. . . . . . . . . . (Re_EstablishmentTimer)re_EstablishmentTimer = 0
. . . . . . . . . RB_InformationSetupList
. . . . . . . . . . RB_InformationSetup
. . . . . . . . . . . (IntegerType)rb_Identity = 20
. . . . . . . . . . . PDCP_Info
. . . . . . . . . . . RLC_InfoChoice
. . . . . . . . . . . . RLC_Info
. . . . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . . . MaxDAT_Retransmissions
. . . . . . . . . . . . . . . . . (MaxDAT)maxDAT = 3
. . . . . . . . . . . . . . . . . (TimerMRW)timerMRW = 13
. . . . . . . . . . . . . . . . . (MaxMRW)maxMRW = 1
. . . . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize = 5
. . . . . . . . . . . . . . . (TimerRST)timerRST = 9
. . . . . . . . . . . . . . . (MaxRST)max_RST = 1
. . . . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit = -
. . . . . . . . . . . . . . . . (TimerPoll)timerPoll = -
. . . . . . . . . . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . . . . . . . . . (Poll_SDU)poll_SDU = 0
. . . . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = FALSE
. . . . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . . . (PollWindow)pollWindow = -
. . . . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize = 5
. . . . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit = -
. . . . . . . . . . . . . . . . (TimerEPC)timerEPC = -
. . . . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . . . . . . . . RB_MappingInfo
. . . . . . . . . . . . RB_MappingOption
. . . . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . . . (IntegerType)dch = 1
. . . . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 7
. . . . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 7
. . . . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . . . (IntegerType)dch = 6
. . . . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 7
. . . . . . . RB_InformationAffectedList
. . . . . . . DL_CounterSynchronisationInfo
. . . . . . . UL_CommonTransChInfo
. . . . . . . . TFC_Subset
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . TFCS
. . . . . . . . . . . ExplicitTFCS_Configuration
. . . . . . . . . . . . TFCS_ReconfAdd
. . . . . . . . . . . . . ctfcSize
. . . . . . . . . . . . . . ctfc4Bit
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . . . . . . . (IntegerType)ctfc4 = 0
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . . . . . . . (IntegerType)ctfc4 = 1
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . . . . . . . (IntegerType)ctfc4 = 2
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . . . . . . . (IntegerType)ctfc4 = 3
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 11
. . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . UL_DeletedTransChInfoList
. . . . . . . UL_AddReconfTransChInfoList
. . . . . . . . UL_AddReconfTransChInformation
. . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType = 0
. . . . . . . . . (IntegerType)transportChannelIdentity = 1
. . . . . . . . . TransportFormatSet
. . . . . . . . . . DedicatedTransChTFS
. . . . . . . . . . . tti
. . . . . . . . . . . . DedicatedDynamicTF_InfoList
. . . . . . . . . . . . . DedicatedDynamicTF_Info
. . . . . . . . . . . . . . rlc_Size
. . . . . . . . . . . . . . . OctetModeRLC_SizeInfoType1
. . . . . . . . . . . . . . . . (IntegerType)sizeType1 = 16
. . . . . . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . LogicalChannelList
. . . . . . . . . . . SemistaticTF_Information
. . . . . . . . . . . . ChannelCodingType
. . . . . . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . . . . . (IntegerType)rateMatchingAttribute = 155
. . . . . . . . . . . . (CRC_Size)crc_Size = 3
. . . . . . . . UL_AddReconfTransChInformation
. . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType = 0
. . . . . . . . . (IntegerType)transportChannelIdentity = 5
. . . . . . . . . TransportFormatSet
. . . . . . . . . . DedicatedTransChTFS
. . . . . . . . . . . tti
. . . . . . . . . . . . DedicatedDynamicTF_InfoList
. . . . . . . . . . . . . DedicatedDynamicTF_Info
. . . . . . . . . . . . . . rlc_Size
. . . . . . . . . . . . . . . BitModeRLC_SizeInfo
. . . . . . . . . . . . . . . . sizeType2
. . . . . . . . . . . . . . . . . (IntegerType)part1 = 2
. . . . . . . . . . . . . . . . . (IntegerType)part2 = -
. . . . . . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . LogicalChannelList
. . . . . . . . . . . SemistaticTF_Information
. . . . . . . . . . . . ChannelCodingType
. . . . . . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . . . . . (IntegerType)rateMatchingAttribute = 170
. . . . . . . . . . . . (CRC_Size)crc_Size = 3
. . . . . . . modeSpecificTransChInfo
. . . . . . . . fdd
. . . . . . . . . (IntegerType)cpch_SetID = -
. . . . . . . . . DRAC_StaticInformationList
. . . . . . . DL_CommonTransChInfo
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . dl_Parameters
. . . . . . . DL_DeletedTransChInfoList
. . . . . . . DL_AddReconfTransChInfoList
. . . . . . . . DL_AddReconfTransChInformation
. . . . . . . . . (DL_TrCH_Type)dl_TransportChannelType = 0
. . . . . . . . . (IntegerType)dl_transportChannelIdentity = 6
. . . . . . . . . tfs_SignallingMode
. . . . . . . . . . UL_TransportChannelIdentity
. . . . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType = 0
. . . . . . . . . . . (IntegerType)ul_TransportChannelIdentity = 1
. . . . . . . . . QualityTarget
. . . . . . . . . . (IntegerType)bler_QualityValue = -20
. . . . . . . . . TM_SignallingInfo
. . . . . . . . DL_AddReconfTransChInformation
. . . . . . . . . (DL_TrCH_Type)dl_TransportChannelType = 0
. . . . . . . . . (IntegerType)dl_transportChannelIdentity = 10
. . . . . . . . . tfs_SignallingMode
. . . . . . . . . . UL_TransportChannelIdentity
. . . . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType = 0
. . . . . . . . . . . (IntegerType)ul_TransportChannelIdentity = 5
. . . . . . . . . QualityTarget
. . . . . . . . . . (IntegerType)bler_QualityValue = -20
. . . . . . . . . TM_SignallingInfo
. . . . . . . FrequencyInfo
. . . . . . . (IntegerType)maxAllowedUL_TX_Power = 33
. . . . . . . UL_ChannelRequirement
. . . . . . . . UL_DPCH_Info
. . . . . . . . . UL_DPCH_PowerControlInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (IntegerType)dpcch_PowerOffset = -40
. . . . . . . . . . . (IntegerType)pc_Preamble = 1
. . . . . . . . . . . (IntegerType)sRB_delay = 7
. . . . . . . . . . . PowerControlAlgorithm
. . . . . . . . . . . . (IntegerType)algorithm1 = 1
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (ScramblingCodeType)scramblingCodeType = 1
. . . . . . . . . . . (IntegerType)scramblingCode = 0
. . . . . . . . . . . (IntegerType)numberOfDPDCH = -
. . . . . . . . . . . (SpreadingFactor)spreadingFactor = 4
. . . . . . . . . . . (BooleanType)tfci_Existence = TRUE
. . . . . . . . . . . (IntegerType)numberOfFBI_Bits = -
. . . . . . . . . . . (PuncturingLimit)puncturingLimit = 15
. . . . . . . modeSpecificPhysChInfo
. . . . . . . . fdd
. . . . . . . . . DL_PDSCH_Information
. . . . . . . DL_CommonInformation
. . . . . . . . DL_DPCH_InfoCommon
. . . . . . . . . cfnHandling
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . DL_DPCH_PowerControlInfo
. . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . (DPC_Mode)dpc_Mode = 0
. . . . . . . . . . . (IntegerType)powerOffsetPilot_pdpdch = 0
. . . . . . . . . . . Dl_rate_matching_restriction
. . . . . . . . . . . SF512_AndPilot
. . . . . . . . . . . . (PilotBits128)sfd128 = 0
. . . . . . . . . . . (PositionFixedOrFlexible)positionFixedOrFlexible = 1
. . . . . . . . . . . (BooleanType)tfci_Existence = TRUE
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . (IntegerType)defaultDPCH_OffsetValue = -
. . . . . . . . . . DPCH_CompressedModeInfo
. . . . . . . . . . (TX_DiversityMode)tx_DiversityMode = 0
. . . . . . . . . . SSDT_Information
. . . . . . . DL_InformationPerRL_List
. . . . . . . . DL_InformationPerRL
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . PrimaryCPICH_Info
. . . . . . . . . . . . (IntegerType)primaryScramblingCode = 100
. . . . . . . . . . . PDSCH_SHO_DCH_Info
. . . . . . . . . . . PDSCH_CodeMapping
. . . . . . . . . DL_DPCH_InfoPerRL
. . . . . . . . . . fdd
. . . . . . . . . . . (PCPICH_UsageForChannelEst)pCPICH_UsageForChannelEst = 0
. . . . . . . . . . . (IntegerType)dpch_FrameOffset = 0
. . . . . . . . . . . SecondaryCPICH_Info
. . . . . . . . . . . DL_ChannelisationCodeList
. . . . . . . . . . . . DL_ChannelisationCode
. . . . . . . . . . . . . (IntegerType)secondaryScramblingCode = 1
. . . . . . . . . . . . . SF512_AndCodeNumber
. . . . . . . . . . . . . . (IntegerType)sf128 = 0
. . . . . . . . . . . . . (ScramblingCodeChange)scramblingCodeChange = -
. . . . . . . . . . . (IntegerType)tpc_CombinationIndex = 0
. . . . . . . . . . . (SSDT_CellIdentity)ssdt_CellIdentity = -
. . . . . . . . . . . (ClosedLoopTimingAdjMode)closedLoopTimingAdjMode = -
. . . . . . . . . SCCPCH_InfoForFACH
. . . . . . v3a0NonCriticalExtensions
. . . . . . . RadioBearerSetup_v3a0ext
. . . . . . . . (BitStringType)new_DSCH_RNTI[16] = -
. . . . . . . laterNonCriticalExtensions
- Constraint:
cas_RB_SetUpAM_WithCnf
- BinaryMessage:
30 4f 02 01 ff 02 01 02 02 01 00 80 00 00 00 03 92 04 ba f2 80 00 16 09 b3 1e 95 92 20 95 11 a0 19 c8 56 20 40 38 24 52 49 32 bf 02 00 82 40 22 39 a6 21 00 88 22 3a 96 0c 30 b0 2b 89 89 5d 34 a8 f4 40 00 00 27 c9 00 ac 40 81 90 00 02 0a 00 00

- No.: 1741
- Timestamp: 20:48:55:526_0
- RFN: 2757
- Chip: 11264
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_CNF
- Source: ts_RRC_SetUpRAB_AM_7_RLC LINE 6
- Message Structure:
RLC_AM_DATA_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. (IntegerType)mui = 0
- Constraint:
car_AM_DataMuiCnf
- BinaryMessage:
30 09 02 01 ff 02 01 02 02 01 00

- No.: 1748
- Timestamp: 20:48:55:659_0
- RFN: 2770
- Chip: 23040
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Modify_REQ
- Source: ts_SS_2DCH_Modify LINE 3
- Message Structure:
CPHY_RL_Modify_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
. (RatType)ratType = 0
. CphyRlModifyReq
. . SS_ActivationTime
. . . (IntegerType)activationCFN = 160
. . physicalChannelInfo
. . . DPCHInfo
. . . . UL_DPCH_Info
. . . . DL_DPCHInfo
. . . . . DL_CommonInformation
. . . . . . DL_DPCH_InfoCommon
. . . . . . . cfnHandling
. . . . . . . modeSpecificInfo
. . . . . . . . fdd
. . . . . . . . . DL_DPCH_PowerControlInfo
. . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . fdd
. . . . . . . . . . . . (DPC_Mode)dpc_Mode = 0
. . . . . . . . . (IntegerType)powerOffsetPilot_pdpdch = 0
. . . . . . . . . Dl_rate_matching_restriction
. . . . . . . . . SF512_AndPilot
. . . . . . . . . . (PilotBits128)sfd128 = 0
. . . . . . . . . (PositionFixedOrFlexible)positionFixedOrFlexible = 1
. . . . . . . . . (BooleanType)tfci_Existence = TRUE
. . . . . . modeSpecificInfo
. . . . . . . fdd
. . . . . . . . (IntegerType)defaultDPCH_OffsetValue = -
. . . . . . . . DPCH_CompressedModeInfo
. . . . . . . . (TX_DiversityMode)tx_DiversityMode = 0
. . . . . . . . SSDT_Information
. . . . . DL_DPCH_InfoPerRL
. . . . . . fdd
. . . . . . . (PCPICH_UsageForChannelEst)pCPICH_UsageForChannelEst = 0
. . . . . . . (IntegerType)dpch_FrameOffset = 0
. . . . . . . SecondaryCPICH_Info
. . . . . . . DL_ChannelisationCodeList
. . . . . . . . DL_ChannelisationCode
. . . . . . . . . (IntegerType)secondaryScramblingCode = 1
. . . . . . . . . SF512_AndCodeNumber
. . . . . . . . . . (IntegerType)sf128 = 0
. . . . . . . . . (ScramblingCodeChange)scramblingCodeChange = -
. . . . . . . (IntegerType)tpc_CombinationIndex = 0
. . . . . . . (SSDT_CellIdentity)ssdt_CellIdentity = -
. . . . . . . (ClosedLoopTimingAdjMode)closedLoopTimingAdjMode = -
. . . . . (IntegerType)powerOffsetOfTFCI_PO1 = 0
. . . . . (IntegerType)powerOffsetOfTPC_PO2 = 0
. . . . . (IntegerType)powerOffsetOfPILOT_PO3 = 0
. . . . . (IntegerType)dl_TxPower = -5
. . . . . (IntegerType)dl_TxPowerMax = 15
. . . . . (IntegerType)dl_TxPowerMin = -35
- Constraint:
ca_DL_DPCH_ModifyInfo
- BinaryMessage:
30 5e 02 01 00 02 01 1a 0a 01 00 30 53 02 02 00 a0 30 4d 30 4b 30 21 30 19 05 00 30 30 14 30 06 30 30 03 0a 01 00 02 01 00 0a 01 00 0a 01 01 01 01 ff 30 30 03 0a 01 00 30 30 13 0a 01 00 02 01 00 30 08 30 06 02 01 01 02 01 00 02 01 00 02 01 00 02 01 00 02 01 00 02 01 fb 02 01 0f 02 01 dd

- No.: 1752
- Timestamp: 20:48:55:707_0
- RFN: 2775
- Chip: 18944
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Modify_CNF
- Source: ts_SS_2DCH_Modify LINE 4
- Message Structure:
CPHY_RL_Modify_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
ca_RL_ModifyCnf
- BinaryMessage:
30 06 02 01 00 02 01 1a

- No.: 1753
- Timestamp: 20:48:55:734_0
- RFN: 2778
- Chip: 7936
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Config_REQ
- Source: ts_SS_2DCH_Modify LINE 5
- Message Structure:
CPHY_TrCH_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
. (RatType)ratType = 0
. CphyTrchConfigReq
. . SS_ActivationTime
. . . (IntegerType)activationCFN = 160
. . ulconnectedTrCHList
. . TFCS
. . dlconnectedTrCHList
. . . CphyTrchConfigReq_setseq_1
. . . . (IntegerType)trchid = 6
. . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 144
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional = 1
. . . . . . (IntegerType)rateMatchingAttribute = 155
. . . . . . (CRC_Size)crc_Size = 3
. . . CphyTrchConfigReq_setseq_1
. . . . (IntegerType)trchid = 10
. . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 148
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional = 1
. . . . . . (IntegerType)rateMatchingAttribute = 170
. . . . . . (CRC_Size)crc_Size = 3
. . TFCS
. . . ExplicitTFCS_Configuration
. . . . TFCS_ReconfAdd
. . . . . ctfcSize
. . . . . . ctfc4Bit
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 0
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 1
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 2
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 3
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . fdd
. . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 9
. . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
- Constraint:
ca_TrChCfgInfo
- BinaryMessage:
30 81 96 02 01 00 02 01 1a 0a 01 00 30 81 8a 02 02 00 a0 30 4c 30 24 02 01 06 0a 01 00 30 1c 30 0e 30 0c 02 02 00 90 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 9b 0a 01 03 30 24 02 01 0a 0a 01 00 30 1c 30 0e 30 0c 02 02 00 94 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 aa 0a 01 03 30 36 30 30 33 30 08 02 01 00 30 03 02 01 00 30 08 02 01 01 30 03 02 01 00 30 08 02 01 02 30 03 02 01 00 30 13 02 01 03 30 0e 30 0c 30 30 03 02 01 09 02 01 0f 02 01 00

- No.: 1757
- Timestamp: 20:48:55:790_0
- RFN: 2783
- Chip: 29696
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Config_CNF
- Source: ts_SS_2DCH_Modify LINE 6
- Message Structure:
CPHY_TrCH_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
ca_TrChCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 1a

- No.: 1758
- Timestamp: 20:48:55:853_0
- RFN: 2789
- Chip: 37376
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_SS_2DCH_Modify LINE 7
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
. (RatType)ratType = 0
. configMessage
. . CmacConfigReq
. . . SS_ActivationTime
. . . . (IntegerType)activationCFN = 160
. . . UE_Info
. . . . U_RNTI
. . . . (BitStringType)c_RNTI[16] = -
. . . TrCHInfo
. . . . ulconnectedTrCHList
. . . . TFCS
. . . . dlconnectedTrCHList
. . . . . TrCHInfo_setseq_1
. . . . . . (IntegerType)trchid = 6
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 144
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . (IntegerType)rateMatchingAttribute = 155
. . . . . . . . (CRC_Size)crc_Size = 3
. . . . . TrCHInfo_setseq_1
. . . . . . (IntegerType)trchid = 10
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 148
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . (IntegerType)rateMatchingAttribute = 170
. . . . . . . . (CRC_Size)crc_Size = 3
. . . . TFCS
. . . . . ExplicitTFCS_Configuration
. . . . . . TFCS_ReconfAdd
. . . . . . . ctfcSize
. . . . . . . . ctfc4Bit
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 0
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 1
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 2
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 3
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 9
. . . . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . TrCH_LogCHMappingList1
. . . . ulconnectedTrCHList
. . . . dlconnectedTrCHList
. . . . . TrCH_LogCHMappingList1_setseq_1
. . . . . . (IntegerType)trchid = 6
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 7
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 5
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 7
. . . . . . . . (IntegerType)rB_Identity = -12
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . TrCH_LogCHMappingList1_setseq_1
. . . . . . (IntegerType)trchid = 10
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 1
. . . . . . . . (IntegerType)rB_Identity = 1
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 2
. . . . . . . . (IntegerType)rB_Identity = 2
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 3
. . . . . . . . (IntegerType)rB_Identity = 3
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 4
. . . . . . . . (IntegerType)rB_Identity = 4
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_CMAC_ReconfigInfo
- BinaryMessage:
30 82 01 22 02 01 ff 02 01 1a 0a 01 00 30 82 01 15 02 02 00 a0 30 00 30 81 80 30 46 30 21 02 01 06 30 1c 30 0e 30 0c 02 02 00 90 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 9b 0a 01 03 30 21 02 01 0a 30 1c 30 0e 30 0c 02 02 00 94 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 aa 0a 01 03 30 36 30 30 33 30 08 02 01 00 30 03 02 01 00 30 08 02 01 01 30 03 02 01 00 30 08 02 01 02 30 03 02 01 00 30 13 02 01 03 30 0e 30 0c 30 30 03 02 01 09 02 01 0f 02 01 00 30 81 89 30 81 86 30 1d 02 01 06 30 18 30 16 30 11 0a 01 00 0a 01 00 02 01 07 0a 01 05 05 00 02 01 07 02 01 f4 30 65 02 01 0a 30 60 30 16 30 11 0a 01 00 0a 01 00 02 01 01 0a 01 04 05 00 02 01 01 02 01 01 30 16 30 11 0a 01 00 0a 01 00 02 01 02 0a 01 04 05 00 02 01 02 02 01 02 30 16 30 11 0a 01 00 0a 01 00 02 01 03 0a 01 04 05 00 02 01 03 02 01 03 30 16 30 11 0a 01 00 0a 01 00 02 01 04 0a 01 04 05 00 02 01 04 02 01 04

- No.: 1762
- Timestamp: 20:48:55:912_0
- RFN: 2795
- Chip: 35072
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_SS_2DCH_Modify LINE 8
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 1a

- No.: 1763
- Timestamp: 20:48:55:939_0
- RFN: 2798
- Chip: 25600
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Modify_REQ
- Source: ts_SS_2DCH_Modify LINE 9
- Message Structure:
CPHY_RL_Modify_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
. (RatType)ratType = 0
. CphyRlModifyReq
. . SS_ActivationTime
. . . (IntegerType)activationCFN = 160
. . physicalChannelInfo
. . . DPCHInfo
. . . . UL_DPCH_Info
. . . . . UL_DPCH_PowerControlInfo
. . . . . . fdd
. . . . . . . (IntegerType)dpcch_PowerOffset = -40
. . . . . . . (IntegerType)pc_Preamble = 1
. . . . . . . (IntegerType)sRB_delay = 7
. . . . . . . PowerControlAlgorithm
. . . . . . . . (IntegerType)algorithm1 = 1
. . . . . modeSpecificInfo
. . . . . . fdd
. . . . . . . (ScramblingCodeType)scramblingCodeType = 1
. . . . . . . (IntegerType)scramblingCode = 0
. . . . . . . (IntegerType)numberOfDPDCH = -
. . . . . . . (SpreadingFactor)spreadingFactor = 4
. . . . . . . (BooleanType)tfci_Existence = TRUE
. . . . . . . (IntegerType)numberOfFBI_Bits = -
. . . . . . . (PuncturingLimit)puncturingLimit = 15
. . . . DL_DPCHInfo
- Constraint:
ca_UL_DPCH_ModifyInfo
- BinaryMessage:
30 34 02 01 00 02 01 14 0a 01 00 30 29 02 02 00 a0 30 23 30 21 30 30 0c 02 01 d8 02 01 01 02 01 07 02 01 01 30 30 0f 0a 01 01 02 01 00 0a 01 04 01 01 ff 0a 01 0f

- No.: 1767
- Timestamp: 20:48:55:988_0
- RFN: 2803
- Chip: 21248
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Modify_CNF
- Source: ts_SS_2DCH_Modify LINE 10
- Message Structure:
CPHY_RL_Modify_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_RL_ModifyCnf
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 1768
- Timestamp: 20:48:56:018_0
- RFN: 2806
- Chip: 20736
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Config_REQ
- Source: ts_SS_2DCH_Modify LINE 11
- Message Structure:
CPHY_TrCH_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
. (RatType)ratType = 0
. CphyTrchConfigReq
. . SS_ActivationTime
. . . (IntegerType)activationCFN = 160
. . ulconnectedTrCHList
. . . CphyTrchConfigReq_setseq_0
. . . . (IntegerType)trchid = 1
. . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 144
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional = 1
. . . . . . (IntegerType)rateMatchingAttribute = 155
. . . . . . (CRC_Size)crc_Size = 3
. . . CphyTrchConfigReq_setseq_0
. . . . (IntegerType)trchid = 5
. . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 148
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional = 1
. . . . . . (IntegerType)rateMatchingAttribute = 170
. . . . . . (CRC_Size)crc_Size = 3
. . TFCS
. . . ExplicitTFCS_Configuration
. . . . TFCS_ReconfAdd
. . . . . ctfcSize
. . . . . . ctfc4Bit
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 0
. . . . . . . . PowerOffsetInformation
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 1
. . . . . . . . PowerOffsetInformation
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 2
. . . . . . . . PowerOffsetInformation
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 3
. . . . . . . . PowerOffsetInformation
. . dlconnectedTrCHList
. . TFCS
- Constraint:
ca_TrChCfgInfo
- BinaryMessage:
30 76 02 01 00 02 01 14 0a 01 00 30 6b 02 02 00 a0 30 4c 30 24 02 01 01 0a 01 00 30 1c 30 0e 30 0c 02 02 00 90 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 9b 0a 01 03 30 24 02 01 05 0a 01 00 30 1c 30 0e 30 0c 02 02 00 94 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 aa 0a 01 03 30 17 30 30 14 30 03 02 01 00 30 03 02 01 01 30 03 02 01 02 30 03 02 01 03

- No.: 1772
- Timestamp: 20:48:56:068_0
- RFN: 2811
- Chip: 23296
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Config_CNF
- Source: ts_SS_2DCH_Modify LINE 12
- Message Structure:
CPHY_TrCH_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_TrChCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 1773
- Timestamp: 20:48:56:133_0
- RFN: 2817
- Chip: 37888
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_SS_2DCH_Modify LINE 13
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
. (RatType)ratType = 0
. configMessage
. . CmacConfigReq
. . . SS_ActivationTime
. . . . (IntegerType)activationCFN = 160
. . . UE_Info
. . . . U_RNTI
. . . . (BitStringType)c_RNTI[16] = -
. . . TrCHInfo
. . . . ulconnectedTrCHList
. . . . . TrCHInfo_setseq_0
. . . . . . (IntegerType)trchid = 1
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 144
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . (IntegerType)rateMatchingAttribute = 155
. . . . . . . . (CRC_Size)crc_Size = 3
. . . . . TrCHInfo_setseq_0
. . . . . . (IntegerType)trchid = 5
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 148
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . (IntegerType)rateMatchingAttribute = 170
. . . . . . . . (CRC_Size)crc_Size = 3
. . . . TFCS
. . . . . ExplicitTFCS_Configuration
. . . . . . TFCS_ReconfAdd
. . . . . . . ctfcSize
. . . . . . . . ctfc4Bit
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 0
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 1
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 2
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 3
. . . . . . . . . . PowerOffsetInformation
. . . . dlconnectedTrCHList
. . . . TFCS
. . . TrCH_LogCHMappingList1
. . . . ulconnectedTrCHList
. . . . . TrCH_LogCHMappingList1_setseq_0
. . . . . . (IntegerType)trchid = 1
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 7
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 5
. . . . . . . . (IntegerType)rB_Identity = -12
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . TrCH_LogCHMappingList1_setseq_0
. . . . . . (IntegerType)trchid = 5
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . (IntegerType)rB_Identity = 1
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . (IntegerType)rB_Identity = 2
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . (IntegerType)rB_Identity = 3
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . (IntegerType)rB_Identity = 4
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . dlconnectedTrCHList
- Constraint:
ca_CMAC_ReconfigInfo
- BinaryMessage:
30 81 e6 02 01 ff 02 01 14 0a 01 00 30 81 da 02 02 00 a0 30 00 30 61 30 46 30 21 02 01 01 30 1c 30 0e 30 0c 02 02 00 90 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 9b 0a 01 03 30 21 02 01 05 30 1c 30 0e 30 0c 02 02 00 94 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 aa 0a 01 03 30 17 30 30 14 30 03 02 01 00 30 03 02 01 01 30 03 02 01 02 30 03 02 01 03 30 6f 30 6d 30 18 02 01 01 30 13 30 11 30 0c 0a 01 00 0a 01 00 02 01 07 0a 01 05 02 01 f4 30 51 02 01 05 30 4c 30 11 30 0c 0a 01 00 0a 01 00 02 01 01 0a 01 04 02 01 01 30 11 30 0c 0a 01 00 0a 01 00 02 01 02 0a 01 04 02 01 02 30 11 30 0c 0a 01 00 0a 01 00 02 01 03 0a 01 04 02 01 03 30 11 30 0c 0a 01 00 0a 01 00 02 01 04 0a 01 04 02 01 04

- No.: 1774
- Timestamp: 20:48:56:163_0
- RFN: 2820
- Chip: 37376
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_SS_2DCH_Modify LINE 14
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 14

- No.: 1777
- Timestamp: 20:48:56:173_0
- RFN: 2822
- Chip: 1024
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB_TM_Cfg_RLC LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = -12
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_TM_RLC_Mode
. . . . . . (BooleanType)segmentationIndication = TRUE
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 144
. . . . . UL_RLC_Mode
. . . . . . UL_TM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . (BooleanType)segmentationIndication = TRUE
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = 7
. . . . (IntegerType)dLlogicalChannelIdentity = 7
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_TM_Info
- BinaryMessage:
30 25 02 01 ff 02 01 f4 0a 01 00 30 1a 30 10 30 03 01 01 ff 30 09 02 02 00 90 30 03 01 01 ff 30 06 02 01 07 02 01 07

- No.: 1781
- Timestamp: 20:48:56:186_0
- RFN: 2823
- Chip: 13056
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB_TM_Cfg_RLC LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = -12
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 f4

- No.: 1789
- Timestamp: 20:48:56:195_0
- RFN: 2824
- Chip: 7424
- Event: Start Timer
- Source: ts_RRC_ReceiveRB_SetupCmpl LINE 2
- Message Structure:
no details available
- Constraint:
t_WaitMS (13500 Ms)
- BinaryMessage:

- No.: 1798
- Timestamp: 20:48:57:821_0
- RFN: 2986
- Chip: 33024
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_IND
- Source: ts_RRC_ReceiveRB_SetupCmpl:lt_CipheringNotStartedAM_RAB LINE 4
- Message Structure:
RLC_AM_DATA_IND
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. IntegrityResult
. . (IntegrityStatus)integrityUsed = 0
. aM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "01100111110100110110111001101110"
. . . . (IntegerType)rrc_MessageSequenceNumber = 2
. . . UL_DCCH_MessageType
. . . . RadioBearerSetupComplete
. . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . IntegrityProtActivationInfo
. . . . . (IntegerType)ul_TimingAdvance = 0
. . . . . (BitStringType)start_Value[20] = "00000000000000000100"
. . . . . (IntegerType)count_C_ActivationTime = 0
. . . . . UL_CounterSynchronisationInfo
. . . . . laterNonCriticalExtensions
. . . . . . (BitStringType)radioBearerSetupComplete_r3_add_ext = 0
. . . . . . nonCriticalExtensions
- Constraint:
car_RB_SetUpCmpl
- BinaryMessage:
30 12 02 01 ff 02 01 02 0a 01 00 b3 e9 b7 37 13 c8 00 00 08

- No.: 1799
- Timestamp: 20:48:57:823_0
- RFN: 2987
- Chip: 256
- Event: Cancel Timer
- Source: ts_RRC_ReceiveRB_SetupCmpl:lt_CipheringNotStartedAM_RAB LINE 4
- Message Structure:
no details available
- Constraint:
t_WaitMS
- BinaryMessage:

- No.: 1800
- Timestamp: 20:48:57:823_1
- RFN: 2987
- Chip: 1024
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ReceiveRB_SetupCmpl:lt_CipheringNotStartedAM_RAB LINE 4
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1825
- Timestamp: 20:48:57:860_0
- RFN: 2990
- Chip: 27136
- Event: Send
- PCO: Dc
- Message: RRC_DataReq
- Source: ts_TC_CloseUE_TestLoop LINE 6
- Message Structure:
RRC_DataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[-1] = -
. (SapId)sapId[1] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. CLOSEUETESTLOOP
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)tCProtocolDiscriminator[4] = '1111'B
. . (MsgType)msgType[8] = '01000000'B
. . (UE_TestLoopMode)uE_TestLoopMode[1] = '00'O
. . UE_TestLoopMode1LB_Setup
. . . (Length)iel[1] = '03'O
. . . LB_SetupRB_IE
. . . . (BitStringType)rLC_SDU_Size[16] = '0000000011111000'B
. . . . (BitStringType)spare_2[3] = '000'B
. . . . (BitStringType)rB_Identity[5] = '10100'B
. . . LB_SetupRB_IE
. . . LB_SetupRB_IE
. . . LB_SetupRB_IE
- Constraint:
ca_PS_DataReq
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 0f 40 00 03 00 f8 14

- No.: 1826
- Timestamp: 20:48:57:861_0
- RFN: 2990
- Chip: 32256
- Event: Start Timer
- Source: ts_TC_CloseUE_TestLoop LINE 6
- Message Structure:
no details available
- Constraint:
t_Dly (5000 Ms)
- BinaryMessage:

- No.: 1830
- Timestamp: 20:48:58:136_0
- RFN: 3018
- Chip: 12288
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_TC_CloseUE_TestLoop LINE 7
- Message Structure:
RRC_DataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. (START_Value)start[0] = -
. CLOSEUETESTLOOPCOMPLETE
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)tCProtocolDiscriminator[4] = '1111'B
. . (MsgType)msgType[8] = '01000001'B
- Constraint:
car_PS_UplinkDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 0f 41

- No.: 1831
- Timestamp: 20:48:58:137_0
- RFN: 3018
- Chip: 15616
- Event: Cancel Timer
- Source: ts_TC_CloseUE_TestLoop LINE 7
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 1832
- Timestamp: 20:48:58:137_1
- RFN: 3018
- Chip: 16384
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_TC_CloseUE_TestLoop LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1839
- Timestamp: 20:48:58:148_1
- RFN: 3019
- Chip: 20736
- Event: Start Timer
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 5
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 1846
- Timestamp: 20:48:58:165_0
- RFN: 3021
- Chip: 7680
- Event: Timeout
- Source: tc_7_2_3_18:lt_TxAndRx LINE 5
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 1866
- Timestamp: 20:48:58:207_0
- RFN: 3025
- Chip: 18688
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000000'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'FFE665A5C5CA3452085408ABEECE4B'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 01 1e ff e6 65 a5 c5 ca 34 52 08 54 08 ab ee ce 4b

- No.: 1875
- Timestamp: 20:48:58:220_1
- RFN: 3026
- Chip: 30464
- Event: Start Timer
- Source: tc_7_2_3_18:lt_TxAndRx LINE 9
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 1876
- Timestamp: 20:48:58:221_0
- RFN: 3026
- Chip: 31488
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1881
- Timestamp: 20:48:58:235_0
- RFN: 3028
- Chip: 8960
- Event: Timeout
- Source: tc_7_2_3_18:lt_TxAndRx LINE 5
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 1901
- Timestamp: 20:48:58:273_0
- RFN: 3032
- Chip: 3840
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000001'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '0B813FD337873F2CD1E29AE91BD6C8'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 09 1e 0b 81 3f d3 37 87 3f 2c d1 e2 9a e9 1b d6 c8

- No.: 1910
- Timestamp: 20:48:58:286_1
- RFN: 3033
- Chip: 15616
- Event: Start Timer
- Source: tc_7_2_3_18:lt_TxAndRx LINE 9
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 1911
- Timestamp: 20:48:58:287_0
- RFN: 3033
- Chip: 16384
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1916
- Timestamp: 20:48:58:305_0
- RFN: 3035
- Chip: 9216
- Event: Timeout
- Source: tc_7_2_3_18:lt_TxAndRx LINE 5
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 1918
- Timestamp: 20:48:58:307_1
- RFN: 3035
- Chip: 19712
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1923
- Timestamp: 20:48:58:359_0
- RFN: 3040
- Chip: 22528
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_18:lt_TxAndRx LINE 3
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000000'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . (AM_Data)data[16] = 'FFE665A5C5CA3452085408ABEECE4BFF'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 00 ff e6 65 a5 c5 ca 34 52 08 54 08 ab ee ce 4b ff

- No.: 1934
- Timestamp: 20:48:58:375_1
- RFN: 3042
- Chip: 7680
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1937
- Timestamp: 20:48:58:382_0
- RFN: 3042
- Chip: 33024
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_18:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000001'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = 'E665A5C5CA3452085408ABEECE4BFF'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 0d 1e e6 65 a5 c5 ca 34 52 08 54 08 ab ee ce 4b ff

- No.: 1942
- Timestamp: 20:48:58:394_0
- RFN: 3044
- Chip: 2816
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: tc_7_2_3_18:lt_CheckPollBit LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. STATUS_PDU
. . (DC_Field)dC_Field[1] = '0'B
. . (CtrlPDU_Type)type[3] = '000'B
. . SuperFields
. . . SUFI_WindowSize
. . . SUFI_List
. . . SUFI_RList
. . . SUFI_Bitmap
. . . SUFI_MRW
. . . SUFI_MRW_ACK
. . . SUFI_NoMore
. . . SUFI_Ack
. . . . (SUFI_Type)type[4] = '0010'B
. . . . (AM_SeqNum)lsn[12] = '000000000010'B
. . (HexStringType)superFieldsAndPadRx[-1] = -
. . (Padding)paddingTx[-1] = '0000000000000000000000000000000'H
- Constraint:
cas_StatusReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 02 00 20 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00

- No.: 1944
- Timestamp: 20:48:58:398_1
- RFN: 3044
- Chip: 18432
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: tc_7_2_3_18:lt_CheckPollBit LINE 5
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1952
- Timestamp: 20:48:58:407_2
- RFN: 3045
- Chip: 16384
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1957
- Timestamp: 20:48:58:438_0
- RFN: 3048
- Chip: 22016
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_18:lt_TxAndRx LINE 3
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000010'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . (AM_Data)data[16] = '0B813FD337873F2CD1E29AE91BD6C80B'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 10 0b 81 3f d3 37 87 3f 2c d1 e2 9a e9 1b d6 c8 0b

- No.: 1968
- Timestamp: 20:48:58:454_2
- RFN: 3050
- Chip: 5632
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1971
- Timestamp: 20:48:58:461_0
- RFN: 3050
- Chip: 30976
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_18:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000011'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '813FD337873F2CD1E29AE91BD6C80B'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 1d 1e 81 3f d3 37 87 3f 2c d1 e2 9a e9 1b d6 c8 0b

- No.: 1976
- Timestamp: 20:48:58:473_0
- RFN: 3052
- Chip: 1536
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: tc_7_2_3_18:lt_CheckPollBit LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. STATUS_PDU
. . (DC_Field)dC_Field[1] = '0'B
. . (CtrlPDU_Type)type[3] = '000'B
. . SuperFields
. . . SUFI_WindowSize
. . . SUFI_List
. . . SUFI_RList
. . . SUFI_Bitmap
. . . SUFI_MRW
. . . SUFI_MRW_ACK
. . . SUFI_NoMore
. . . SUFI_Ack
. . . . (SUFI_Type)type[4] = '0010'B
. . . . (AM_SeqNum)lsn[12] = '000000000100'B
. . (HexStringType)superFieldsAndPadRx[-1] = -
. . (Padding)paddingTx[-1] = '0000000000000000000000000000000'H
- Constraint:
cas_StatusReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 02 00 40 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00

- No.: 1978
- Timestamp: 20:48:58:477_0
- RFN: 3052
- Chip: 15616
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: tc_7_2_3_18:lt_CheckPollBit LINE 5
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1988
- Timestamp: 20:48:58:492_0
- RFN: 3053
- Chip: 35328
- Event: Cancel Timer
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 8
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 1992
- Timestamp: 20:48:58:500_0
- RFN: 3054
- Chip: 29952
- Event: Send
- PCO: Dc
- Message: RRC_DataReq
- Source: ts_TC_OpenUE_TestLoop LINE 6
- Message Structure:
RRC_DataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[-1] = -
. (SapId)sapId[1] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. OPENUETESTLOOP
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)tCProtocolDiscriminator[4] = '1111'B
. . (MsgType)msgType[8] = '01000010'B
- Constraint:
ca_PS_DataReq
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 0f 42

- No.: 1993
- Timestamp: 20:48:58:501_0
- RFN: 3054
- Chip: 33536
- Event: Start Timer
- Source: ts_TC_OpenUE_TestLoop LINE 6
- Message Structure:
no details available
- Constraint:
t_Dly (5000 Ms)
- BinaryMessage:

- No.: 1997
- Timestamp: 20:48:58:776_0
- RFN: 3082
- Chip: 11776
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_TC_OpenUE_TestLoop LINE 7
- Message Structure:
RRC_DataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. (START_Value)start[0] = -
. OPENUETESTLOOPCOMPLETE
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)tCProtocolDiscriminator[4] = '1111'B
. . (MsgType)msgType[8] = '01000011'B
- Constraint:
car_PS_UplinkDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 0f 43

- No.: 1998
- Timestamp: 20:48:58:777_0
- RFN: 3082
- Chip: 15104
- Event: Cancel Timer
- Source: ts_TC_OpenUE_TestLoop LINE 7
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 1999
- Timestamp: 20:48:58:777_1
- RFN: 3082
- Chip: 15872
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_TC_OpenUE_TestLoop LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2017
- Timestamp: 20:48:58:786_0
- RFN: 3083
- Chip: 11008
- Event: Send
- PCO: CPHY
- Message: CPHY_Frame_Number_REQ
- Source: ts_CPHY_ActTime LINE 1
- Message Structure:
CPHY_Frame_Number_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
cas_GetFrameNum
- BinaryMessage:
30 06 02 01 00 02 01 1a

- No.: 2021
- Timestamp: 20:48:58:792_0
- RFN: 3083
- Chip: 37888
- Event: Receive
- PCO: CPHY
- Message: CPHY_Frame_Number_CNF
- Source: ts_CPHY_ActTime LINE 2
- Message Structure:
CPHY_Frame_Number_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
. (IntegerType)frameNumber = 11
- Constraint:
car_GetFrameNum
- BinaryMessage:
30 09 02 01 00 02 01 1a 02 01 0b

- No.: 2027
- Timestamp: 20:48:58:820_0
- RFN: 3086
- Chip: 28672
- Event: Send
- PCO: AM
- Message: RLC_AM_DATA_REQ
- Source: ts_RRC_RB_RelRLC:lt_SendRAB_Rel LINE 4
- Message Structure:
RLC_AM_DATA_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. AmConfirmationRequest
. aM_message
. . DL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00000000000000000000000000000000"
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . DL_DCCH_MessageType
. . . . RadioBearerRelease
. . . . . r3
. . . . . . RadioBearerRelease_r3_IEs
. . . . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . . . IntegrityProtectionModeInfo
. . . . . . . CipheringModeInfo
. . . . . . . (IntegerType)activationTime = 0
. . . . . . . U_RNTI
. . . . . . . (BitStringType)new_C_RNTI[16] = -
. . . . . . . (RRC_StateIndicator)rrc_StateIndicator = 0
. . . . . . . (IntegerType)utran_DRX_CycleLengthCoeff = -
. . . . . . . CN_InformationInfo
. . . . . . . (CN_DomainIdentity)signallingConnectionRelIndication = -
. . . . . . . (BitStringType)ura_Identity[16] = -
. . . . . . . RAB_InformationReconfigList
. . . . . . . RB_InformationReleaseList
. . . . . . . . (IntegerType)_elem = 20
. . . . . . . RB_InformationAffectedList
. . . . . . . DL_CounterSynchronisationInfo
. . . . . . . UL_CommonTransChInfo
. . . . . . . . TFC_Subset
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . TFCS
. . . . . . . . . . . ExplicitTFCS_Configuration
. . . . . . . . . . . . TFCS_ReconfAdd
. . . . . . . . . . . . . ctfcSize
. . . . . . . . . . . . . . ctfc2Bit
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . . . . . . . (IntegerType)ctfc2 = 0
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . . . . . . . (IntegerType)ctfc2 = 1
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 11
. . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . UL_DeletedTransChInfoList
. . . . . . . . UL_TransportChannelIdentity
. . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType = 0
. . . . . . . . . (IntegerType)ul_TransportChannelIdentity = 1
. . . . . . . UL_AddReconfTransChInfoList
. . . . . . . . UL_AddReconfTransChInformation
. . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType = 0
. . . . . . . . . (IntegerType)transportChannelIdentity = 5
. . . . . . . . . TransportFormatSet
. . . . . . . . . . DedicatedTransChTFS
. . . . . . . . . . . tti
. . . . . . . . . . . . DedicatedDynamicTF_InfoList
. . . . . . . . . . . . . DedicatedDynamicTF_Info
. . . . . . . . . . . . . . rlc_Size
. . . . . . . . . . . . . . . BitModeRLC_SizeInfo
. . . . . . . . . . . . . . . . sizeType2
. . . . . . . . . . . . . . . . . (IntegerType)part1 = 2
. . . . . . . . . . . . . . . . . (IntegerType)part2 = -
. . . . . . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . LogicalChannelList
. . . . . . . . . . . SemistaticTF_Information
. . . . . . . . . . . . ChannelCodingType
. . . . . . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . . . . . (IntegerType)rateMatchingAttribute = 192
. . . . . . . . . . . . (CRC_Size)crc_Size = 3
. . . . . . . modeSpecificTransChInfo
. . . . . . . . fdd
. . . . . . . . . (IntegerType)cpch_SetID = -
. . . . . . . . . DRAC_StaticInformationList
. . . . . . . DL_CommonTransChInfo
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . dl_Parameters
. . . . . . . DL_DeletedTransChInfoList
. . . . . . . . DL_TransportChannelIdentity
. . . . . . . . . (DL_TrCH_Type)dl_TransportChannelType = 0
. . . . . . . . . (IntegerType)dl_TransportChannelIdentity = 6
. . . . . . . DL_AddReconfTransChInfo2List
. . . . . . . . DL_AddReconfTransChInformation2
. . . . . . . . . (DL_TrCH_Type)dl_TransportChannelType = 0
. . . . . . . . . (IntegerType)transportChannelIdentity = 10
. . . . . . . . . tfs_SignallingMode
. . . . . . . . . . UL_TransportChannelIdentity
. . . . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType = 0
. . . . . . . . . . . (IntegerType)ul_TransportChannelIdentity = 5
. . . . . . . . . QualityTarget
. . . . . . . FrequencyInfo
. . . . . . . . modeSpecificInfo
. . . . . . . . . FrequencyInfoFDD
. . . . . . . . . . (IntegerType)uarfcn_UL = -
. . . . . . . . . . (IntegerType)uarfcn_DL = 10700
. . . . . . . (IntegerType)maxAllowedUL_TX_Power = 33
. . . . . . . UL_ChannelRequirement
. . . . . . . . UL_DPCH_Info
. . . . . . . . . UL_DPCH_PowerControlInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (IntegerType)dpcch_PowerOffset = -40
. . . . . . . . . . . (IntegerType)pc_Preamble = 1
. . . . . . . . . . . (IntegerType)sRB_delay = 7
. . . . . . . . . . . PowerControlAlgorithm
. . . . . . . . . . . . (IntegerType)algorithm1 = 1
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (ScramblingCodeType)scramblingCodeType = 1
. . . . . . . . . . . (IntegerType)scramblingCode = 0
. . . . . . . . . . . (IntegerType)numberOfDPDCH = -
. . . . . . . . . . . (SpreadingFactor)spreadingFactor = 4
. . . . . . . . . . . (BooleanType)tfci_Existence = TRUE
. . . . . . . . . . . (IntegerType)numberOfFBI_Bits = -
. . . . . . . . . . . (PuncturingLimit)puncturingLimit = 15
. . . . . . . modeSpecificPhysChInfo
. . . . . . . . fdd
. . . . . . . . . DL_PDSCH_Information
. . . . . . . DL_CommonInformation
. . . . . . . . DL_DPCH_InfoCommon
. . . . . . . . . cfnHandling
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . DL_DPCH_PowerControlInfo
. . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . (DPC_Mode)dpc_Mode = 0
. . . . . . . . . . . (IntegerType)powerOffsetPilot_pdpdch = 0
. . . . . . . . . . . Dl_rate_matching_restriction
. . . . . . . . . . . SF512_AndPilot
. . . . . . . . . . . . (PilotBits128)sfd128 = 0
. . . . . . . . . . . (PositionFixedOrFlexible)positionFixedOrFlexible = 0
. . . . . . . . . . . (BooleanType)tfci_Existence = FALSE
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . (IntegerType)defaultDPCH_OffsetValue = -
. . . . . . . . . . DPCH_CompressedModeInfo
. . . . . . . . . . (TX_DiversityMode)tx_DiversityMode = 0
. . . . . . . . . . SSDT_Information
. . . . . . . DL_InformationPerRL_List
. . . . . . . . DL_InformationPerRL
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . PrimaryCPICH_Info
. . . . . . . . . . . . (IntegerType)primaryScramblingCode = 100
. . . . . . . . . . . PDSCH_SHO_DCH_Info
. . . . . . . . . . . PDSCH_CodeMapping
. . . . . . . . . DL_DPCH_InfoPerRL
. . . . . . . . . . fdd
. . . . . . . . . . . (PCPICH_UsageForChannelEst)pCPICH_UsageForChannelEst = 0
. . . . . . . . . . . (IntegerType)dpch_FrameOffset = 0
. . . . . . . . . . . SecondaryCPICH_Info
. . . . . . . . . . . DL_ChannelisationCodeList
. . . . . . . . . . . . DL_ChannelisationCode
. . . . . . . . . . . . . (IntegerType)secondaryScramblingCode = 1
. . . . . . . . . . . . . SF512_AndCodeNumber
. . . . . . . . . . . . . . (IntegerType)sf128 = 0
. . . . . . . . . . . . . (ScramblingCodeChange)scramblingCodeChange = -
. . . . . . . . . . . (IntegerType)tpc_CombinationIndex = 0
. . . . . . . . . . . (SSDT_CellIdentity)ssdt_CellIdentity = -
. . . . . . . . . . . (ClosedLoopTimingAdjMode)closedLoopTimingAdjMode = -
. . . . . . . . . SCCPCH_InfoForFACH
. . . . . . v3a0NonCriticalExtensions
. . . . . . . RadioBearerRelease_v3a0ext
. . . . . . . . (BitStringType)new_DSCH_RNTI[16] = -
. . . . . . . laterNonCriticalExtensions
- Constraint:
cas_RB_Release
- BinaryMessage:
30 3a 02 01 ff 02 01 02 05 00 80 00 00 00 03 52 00 ff f0 00 04 c8 00 06 25 2b f0 00 00 40 01 10 44 77 ec 18 05 00 98 85 39 94 d2 a3 d1 00 00 00 9f 24 02 81 02 06 40 00 08 28 00 00

- No.: 2038
- Timestamp: 20:48:58:837_0
- RFN: 3088
- Chip: 17920
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = -12
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 f4 0a 01 00 05 00

- No.: 2042
- Timestamp: 20:48:58:844_0
- RFN: 3089
- Chip: 4096
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = -12
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 f4

- No.: 2051
- Timestamp: 20:48:58:856_0
- RFN: 3090
- Chip: 12288
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Modify_REQ
- Source: ts_SS_1DCH_DCCH_Modify LINE 4
- Message Structure:
CPHY_RL_Modify_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
. (RatType)ratType = 0
. CphyRlModifyReq
. . SS_ActivationTime
. . . (IntegerType)activationCFN = 0
. . physicalChannelInfo
. . . DPCHInfo
. . . . UL_DPCH_Info
. . . . DL_DPCHInfo
. . . . . DL_CommonInformation
. . . . . . DL_DPCH_InfoCommon
. . . . . . . cfnHandling
. . . . . . . . initialise
. . . . . . . . . (IntegerType)cfntargetsfnframeoffset = -
. . . . . . . modeSpecificInfo
. . . . . . . . fdd
. . . . . . . . . DL_DPCH_PowerControlInfo
. . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . fdd
. . . . . . . . . . . . (DPC_Mode)dpc_Mode = 0
. . . . . . . . . (IntegerType)powerOffsetPilot_pdpdch = 0
. . . . . . . . . Dl_rate_matching_restriction
. . . . . . . . . SF512_AndPilot
. . . . . . . . . . (PilotBits128)sfd128 = 0
. . . . . . . . . (PositionFixedOrFlexible)positionFixedOrFlexible = 0
. . . . . . . . . (BooleanType)tfci_Existence = FALSE
. . . . . . modeSpecificInfo
. . . . . . . fdd
. . . . . . . . (IntegerType)defaultDPCH_OffsetValue = 0
. . . . . . . . DPCH_CompressedModeInfo
. . . . . . . . (TX_DiversityMode)tx_DiversityMode = 0
. . . . . . . . SSDT_Information
. . . . . DL_DPCH_InfoPerRL
. . . . . . fdd
. . . . . . . (PCPICH_UsageForChannelEst)pCPICH_UsageForChannelEst = 0
. . . . . . . (IntegerType)dpch_FrameOffset = 0
. . . . . . . SecondaryCPICH_Info
. . . . . . . DL_ChannelisationCodeList
. . . . . . . . DL_ChannelisationCode
. . . . . . . . . (IntegerType)secondaryScramblingCode = 1
. . . . . . . . . SF512_AndCodeNumber
. . . . . . . . . . (IntegerType)sf128 = 0
. . . . . . . . . (ScramblingCodeChange)scramblingCodeChange = -
. . . . . . . (IntegerType)tpc_CombinationIndex = 0
. . . . . . . (SSDT_CellIdentity)ssdt_CellIdentity = -
. . . . . . . (ClosedLoopTimingAdjMode)closedLoopTimingAdjMode = -
. . . . . (IntegerType)powerOffsetOfTFCI_PO1 = 0
. . . . . (IntegerType)powerOffsetOfTPC_PO2 = 0
. . . . . (IntegerType)powerOffsetOfPILOT_PO3 = 0
. . . . . (IntegerType)dl_TxPower = -5
. . . . . (IntegerType)dl_TxPowerMax = 15
. . . . . (IntegerType)dl_TxPowerMin = -35
- Constraint:
ca_DL_DPCH_ModifyInfo
- BinaryMessage:
30 61 02 01 00 02 01 1a 0a 01 00 30 56 02 01 00 30 51 30 4f 30 25 30 1a 30 30 00 30 30 14 30 06 30 30 03 0a 01 00 02 01 00 0a 01 00 0a 01 00 01 01 00 30 30 06 02 01 00 0a 01 00 30 30 13 0a 01 00 02 01 00 30 08 30 06 02 01 01 02 01 00 02 01 00 02 01 00 02 01 00 02 01 00 02 01 fb 02 01 0f 02 01 dd

- No.: 2055
- Timestamp: 20:48:58:863_0
- RFN: 3091
- Chip: 768
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Modify_CNF
- Source: ts_SS_1DCH_DCCH_Modify LINE 5
- Message Structure:
CPHY_RL_Modify_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
ca_RL_ModifyCnf
- BinaryMessage:
30 06 02 01 00 02 01 1a

- No.: 2056
- Timestamp: 20:48:58:874_0
- RFN: 3092
- Chip: 7680
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Config_REQ
- Source: ts_SS_1DCH_DCCH_Modify LINE 6
- Message Structure:
CPHY_TrCH_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
. (RatType)ratType = 0
. CphyTrchConfigReq
. . SS_ActivationTime
. . . (IntegerType)activationCFN = 0
. . ulconnectedTrCHList
. . TFCS
. . dlconnectedTrCHList
. . . CphyTrchConfigReq_setseq_1
. . . . (IntegerType)trchid = 10
. . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 148
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional = 1
. . . . . . (IntegerType)rateMatchingAttribute = 192
. . . . . . (CRC_Size)crc_Size = 3
. . TFCS
. . . ExplicitTFCS_Configuration
. . . . TFCS_ReconfAdd
. . . . . ctfcSize
. . . . . . ctfc2Bit
. . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . (IntegerType)ctfc2 = 0
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . (IntegerType)ctfc2 = 1
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . fdd
. . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 11
. . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
- Constraint:
ca_DCH_148_TTI_10_DL_Info
- BinaryMessage:
30 5a 02 01 00 02 01 1a 0a 01 00 30 4f 02 01 00 30 26 30 24 02 01 0a 0a 01 00 30 1c 30 0e 30 0c 02 02 00 94 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 c0 0a 01 03 30 22 30 30 1f 30 08 02 01 00 30 03 02 01 00 30 13 02 01 01 30 0e 30 0c 30 30 03 02 01 0b 02 01 0f 02 01 00

- No.: 2060
- Timestamp: 20:48:58:886_0
- RFN: 3093
- Chip: 12288
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Config_CNF
- Source: ts_SS_1DCH_DCCH_Modify LINE 7
- Message Structure:
CPHY_TrCH_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
ca_TrChCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 1a

- No.: 2061
- Timestamp: 20:48:58:931_0
- RFN: 3097
- Chip: 34816
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_SS_1DCH_DCCH_Modify LINE 8
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
. (RatType)ratType = 0
. configMessage
. . CmacConfigReq
. . . SS_ActivationTime
. . . . (IntegerType)activationCFN = 0
. . . UE_Info
. . . . U_RNTI
. . . . (BitStringType)c_RNTI[16] = -
. . . TrCHInfo
. . . . ulconnectedTrCHList
. . . . TFCS
. . . . dlconnectedTrCHList
. . . . . TrCHInfo_setseq_1
. . . . . . (IntegerType)trchid = 10
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 148
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . (IntegerType)rateMatchingAttribute = 192
. . . . . . . . (CRC_Size)crc_Size = 3
. . . . TFCS
. . . . . ExplicitTFCS_Configuration
. . . . . . TFCS_ReconfAdd
. . . . . . . ctfcSize
. . . . . . . . ctfc2Bit
. . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . (IntegerType)ctfc2 = 0
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . (IntegerType)ctfc2 = 1
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 11
. . . . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . TrCH_LogCHMappingList1
. . . . ulconnectedTrCHList
. . . . dlconnectedTrCHList
. . . . . TrCH_LogCHMappingList1_setseq_1
. . . . . . (IntegerType)trchid = 10
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 1
. . . . . . . . (IntegerType)rB_Identity = 1
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 2
. . . . . . . . (IntegerType)rB_Identity = 2
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 3
. . . . . . . . (IntegerType)rB_Identity = 3
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 4
. . . . . . . . (IntegerType)rB_Identity = 4
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_CMAC_ReconfigInfo
- BinaryMessage:
30 81 c7 02 01 ff 02 01 1a 0a 01 00 30 81 bb 02 01 00 30 00 30 49 30 23 30 21 02 01 0a 30 1c 30 0e 30 0c 02 02 00 94 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 c0 0a 01 03 30 22 30 30 1f 30 08 02 01 00 30 03 02 01 00 30 13 02 01 01 30 0e 30 0c 30 30 03 02 01 0b 02 01 0f 02 01 00 30 69 30 67 30 65 02 01 0a 30 60 30 16 30 11 0a 01 00 0a 01 00 02 01 01 0a 01 04 05 00 02 01 01 02 01 01 30 16 30 11 0a 01 00 0a 01 00 02 01 02 0a 01 04 05 00 02 01 02 02 01 02 30 16 30 11 0a 01 00 0a 01 00 02 01 03 0a 01 04 05 00 02 01 03 02 01 03 30 16 30 11 0a 01 00 0a 01 00 02 01 04 0a 01 04 05 00 02 01 04 02 01 04

- No.: 2062
- Timestamp: 20:48:58:941_0
- RFN: 3098
- Chip: 31744
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_SS_1DCH_DCCH_Modify LINE 9
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 1a

- No.: 2063
- Timestamp: 20:48:58:947_0
- RFN: 3099
- Chip: 15360
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Modify_REQ
- Source: ts_SS_1DCH_DCCH_Modify LINE 10
- Message Structure:
CPHY_RL_Modify_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
. (RatType)ratType = 0
. CphyRlModifyReq
. . SS_ActivationTime
. . . (IntegerType)activationCFN = 0
. . physicalChannelInfo
. . . DPCHInfo
. . . . UL_DPCH_Info
. . . . . UL_DPCH_PowerControlInfo
. . . . . . fdd
. . . . . . . (IntegerType)dpcch_PowerOffset = -40
. . . . . . . (IntegerType)pc_Preamble = 1
. . . . . . . (IntegerType)sRB_delay = 7
. . . . . . . PowerControlAlgorithm
. . . . . . . . (IntegerType)algorithm1 = 1
. . . . . modeSpecificInfo
. . . . . . fdd
. . . . . . . (ScramblingCodeType)scramblingCodeType = 1
. . . . . . . (IntegerType)scramblingCode = 0
. . . . . . . (IntegerType)numberOfDPDCH = -
. . . . . . . (SpreadingFactor)spreadingFactor = 4
. . . . . . . (BooleanType)tfci_Existence = TRUE
. . . . . . . (IntegerType)numberOfFBI_Bits = -
. . . . . . . (PuncturingLimit)puncturingLimit = 15
. . . . DL_DPCHInfo
- Constraint:
ca_UL_DPCH_ModifyInfo
- BinaryMessage:
30 33 02 01 00 02 01 14 0a 01 00 30 28 02 01 00 30 23 30 21 30 30 0c 02 01 d8 02 01 01 02 01 07 02 01 01 30 30 0f 0a 01 01 02 01 00 0a 01 04 01 01 ff 0a 01 0f

- No.: 2067
- Timestamp: 20:48:58:956_0
- RFN: 3100
- Chip: 11008
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Modify_CNF
- Source: ts_SS_1DCH_DCCH_Modify LINE 11
- Message Structure:
CPHY_RL_Modify_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_RL_ModifyCnf
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 2068
- Timestamp: 20:48:58:966_0
- RFN: 3101
- Chip: 9216
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Config_REQ
- Source: ts_SS_1DCH_DCCH_Modify LINE 12
- Message Structure:
CPHY_TrCH_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
. (RatType)ratType = 0
. CphyTrchConfigReq
. . SS_ActivationTime
. . . (IntegerType)activationCFN = 0
. . ulconnectedTrCHList
. . . CphyTrchConfigReq_setseq_0
. . . . (IntegerType)trchid = 5
. . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 148
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional = 1
. . . . . . (IntegerType)rateMatchingAttribute = 192
. . . . . . (CRC_Size)crc_Size = 3
. . TFCS
. . . ExplicitTFCS_Configuration
. . . . TFCS_ReconfAdd
. . . . . ctfcSize
. . . . . . ctfc2Bit
. . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . (IntegerType)ctfc2 = 0
. . . . . . . . PowerOffsetInformation
. . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . (IntegerType)ctfc2 = 1
. . . . . . . . PowerOffsetInformation
. . dlconnectedTrCHList
. . TFCS
- Constraint:
ca_DCH_148_TTI_10_UL_Info
- BinaryMessage:
30 45 02 01 00 02 01 14 0a 01 00 30 3a 02 01 00 30 26 30 24 02 01 05 0a 01 00 30 1c 30 0e 30 0c 02 02 00 94 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 c0 0a 01 03 30 0d 30 30 0a 30 03 02 01 00 30 03 02 01 01

- No.: 2072
- Timestamp: 20:48:58:976_0
- RFN: 3102
- Chip: 9728
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Config_CNF
- Source: ts_SS_1DCH_DCCH_Modify LINE 13
- Message Structure:
CPHY_TrCH_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_TrChCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 2073
- Timestamp: 20:48:59:012_0
- RFN: 3105
- Chip: 35072
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_SS_1DCH_DCCH_Modify LINE 14
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
. (RatType)ratType = 0
. configMessage
. . CmacConfigReq
. . . SS_ActivationTime
. . . . (IntegerType)activationCFN = 0
. . . UE_Info
. . . . U_RNTI
. . . . (BitStringType)c_RNTI[16] = -
. . . TrCHInfo
. . . . ulconnectedTrCHList
. . . . . TrCHInfo_setseq_0
. . . . . . (IntegerType)trchid = 5
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 148
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . (IntegerType)rateMatchingAttribute = 192
. . . . . . . . (CRC_Size)crc_Size = 3
. . . . TFCS
. . . . . ExplicitTFCS_Configuration
. . . . . . TFCS_ReconfAdd
. . . . . . . ctfcSize
. . . . . . . . ctfc2Bit
. . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . (IntegerType)ctfc2 = 0
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . (IntegerType)ctfc2 = 1
. . . . . . . . . . PowerOffsetInformation
. . . . dlconnectedTrCHList
. . . . TFCS
. . . TrCH_LogCHMappingList1
. . . . ulconnectedTrCHList
. . . . . TrCH_LogCHMappingList1_setseq_0
. . . . . . (IntegerType)trchid = 5
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . (IntegerType)rB_Identity = 1
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . (IntegerType)rB_Identity = 2
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . (IntegerType)rB_Identity = 3
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . (IntegerType)rB_Identity = 4
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . dlconnectedTrCHList
- Constraint:
ca_CMAC_ReconfigInfo
- BinaryMessage:
30 81 9e 02 01 ff 02 01 14 0a 01 00 30 81 92 02 01 00 30 00 30 34 30 23 30 21 02 01 05 30 1c 30 0e 30 0c 02 02 00 94 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 c0 0a 01 03 30 0d 30 30 0a 30 03 02 01 00 30 03 02 01 01 30 55 30 53 30 51 02 01 05 30 4c 30 11 30 0c 0a 01 00 0a 01 00 02 01 01 0a 01 04 02 01 01 30 11 30 0c 0a 01 00 0a 01 00 02 01 02 0a 01 04 02 01 02 30 11 30 0c 0a 01 00 0a 01 00 02 01 03 0a 01 04 02 01 03 30 11 30 0c 0a 01 00 0a 01 00 02 01 04 0a 01 04 02 01 04

- No.: 2074
- Timestamp: 20:48:59:020_0
- RFN: 3106
- Chip: 25600
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_SS_1DCH_DCCH_Modify LINE 15
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 14

- No.: 2084
- Timestamp: 20:48:59:022_2
- RFN: 3106
- Chip: 36352
- Event: Start Timer
- Source: ts_RRC_ReceiveRB_RelCmpl LINE 2
- Message Structure:
no details available
- Constraint:
t_WaitMS (13500 Ms)
- BinaryMessage:

- No.: 2088
- Timestamp: 20:49:01:305_0
- RFN: 3335
- Chip: 9728
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_IND
- Source: ts_RRC_ReceiveRB_RelCmpl LINE 3
- Message Structure:
RLC_AM_DATA_IND
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. IntegrityResult
. . (IntegrityStatus)integrityUsed = 0
. aM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "11100111101110000111111101010101"
. . . . (IntegerType)rrc_MessageSequenceNumber = 3
. . . UL_DCCH_MessageType
. . . . RadioBearerReleaseComplete
. . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . IntegrityProtActivationInfo
. . . . . (IntegerType)ul_TimingAdvance = 0
. . . . . (IntegerType)count_C_ActivationTime = 0
. . . . . UL_CounterSynchronisationInfo
. . . . . laterNonCriticalExtensions
. . . . . . (BitStringType)radioBearerReleaseComplete_r3_add_ext = 0
. . . . . . nonCriticalExtensions
- Constraint:
car_RB_RelCmpl
- BinaryMessage:
30 10 02 01 ff 02 01 02 0a 01 00 f3 dc 3f aa 9b 40 00

- No.: 2089
- Timestamp: 20:49:01:307_0
- RFN: 3335
- Chip: 15104
- Event: Cancel Timer
- Source: ts_RRC_ReceiveRB_RelCmpl LINE 3
- Message Structure:
no details available
- Constraint:
t_WaitMS
- BinaryMessage:

- No.: 2090
- Timestamp: 20:49:01:307_1
- RFN: 3335
- Chip: 16128
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ReceiveRB_RelCmpl LINE 3
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2119
- Timestamp: 20:49:01:335_0
- RFN: 3338
- Chip: 9216
- Event: Send
- PCO: CPHY
- Message: CPHY_Frame_Number_REQ
- Source: ts_RRC_SetUpRAB_AM_7_RLC LINE 2
- Message Structure:
CPHY_Frame_Number_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
cas_GetFrameNum
- BinaryMessage:
30 06 02 01 00 02 01 1a

- No.: 2123
- Timestamp: 20:49:01:344_0
- RFN: 3339
- Chip: 6144
- Event: Receive
- PCO: CPHY
- Message: CPHY_Frame_Number_CNF
- Source: ts_RRC_SetUpRAB_AM_7_RLC LINE 3
- Message Structure:
CPHY_Frame_Number_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
. (IntegerType)frameNumber = 10
- Constraint:
car_GetFrameNum
- BinaryMessage:
30 09 02 01 00 02 01 1a 02 01 0a

- No.: 2127
- Timestamp: 20:49:01:390_0
- RFN: 3343
- Chip: 28672
- Event: Send
- PCO: AM
- Message: RLC_AM_DATA_REQ
- Source: ts_RRC_SetUpRAB_AM_7_RLC:lt_SendRAB_SetupCS_OrPS LINE 4
- Message Structure:
RLC_AM_DATA_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. AmConfirmationRequest
. . (IntegerType)confirmationRequested = 0
. aM_message
. . DL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00000000000000000000000000000000"
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . DL_DCCH_MessageType
. . . . RadioBearerSetup
. . . . . r3
. . . . . . RadioBearerSetup_r3_IEs
. . . . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . . . IntegrityProtectionModeInfo
. . . . . . . CipheringModeInfo
. . . . . . . (IntegerType)activationTime = 0
. . . . . . . U_RNTI
. . . . . . . (BitStringType)new_C_RNTI[16] = -
. . . . . . . (RRC_StateIndicator)rrc_StateIndicator = 0
. . . . . . . (IntegerType)utran_DRX_CycleLengthCoeff = -
. . . . . . . (BitStringType)ura_Identity[0] = -
. . . . . . . CN_InformationInfo
. . . . . . . SRB_InformationSetupList
. . . . . . . RAB_InformationSetupList
. . . . . . . . RAB_InformationSetup
. . . . . . . . . RAB_Info
. . . . . . . . . . RAB_Identity
. . . . . . . . . . . (BitStringType)gsm_MAP_RAB_Identity[8] = '00000101'B
. . . . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = 1
. . . . . . . . . . (BitStringType)nas_Synchronisation_Indicator[0] = -
. . . . . . . . . . (Re_EstablishmentTimer)re_EstablishmentTimer = 0
. . . . . . . . . RB_InformationSetupList
. . . . . . . . . . RB_InformationSetup
. . . . . . . . . . . (IntegerType)rb_Identity = 20
. . . . . . . . . . . PDCP_Info
. . . . . . . . . . . RLC_InfoChoice
. . . . . . . . . . . . RLC_Info
. . . . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . . . MaxDAT_Retransmissions
. . . . . . . . . . . . . . . . . (MaxDAT)maxDAT = 3
. . . . . . . . . . . . . . . . . (TimerMRW)timerMRW = 13
. . . . . . . . . . . . . . . . . (MaxMRW)maxMRW = 1
. . . . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize = 6
. . . . . . . . . . . . . . . (TimerRST)timerRST = 9
. . . . . . . . . . . . . . . (MaxRST)max_RST = 1
. . . . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit = -
. . . . . . . . . . . . . . . . (TimerPoll)timerPoll = -
. . . . . . . . . . . . . . . . (Poll_PDU)poll_PDU = -
. . . . . . . . . . . . . . . . (Poll_SDU)poll_SDU = 2
. . . . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = FALSE
. . . . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . . . (PollWindow)pollWindow = -
. . . . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic = -
. . . . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize = 5
. . . . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit = -
. . . . . . . . . . . . . . . . (TimerEPC)timerEPC = -
. . . . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic = -
. . . . . . . . . . . RB_MappingInfo
. . . . . . . . . . . . RB_MappingOption
. . . . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . . . (IntegerType)dch = 1
. . . . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 7
. . . . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 7
. . . . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . . . (IntegerType)dch = 6
. . . . . . . . . . . . . . . (IntegerType)logicalChannelIdentity = 7
. . . . . . . RB_InformationAffectedList
. . . . . . . DL_CounterSynchronisationInfo
. . . . . . . UL_CommonTransChInfo
. . . . . . . . TFC_Subset
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . TFCS
. . . . . . . . . . . ExplicitTFCS_Configuration
. . . . . . . . . . . . TFCS_ReconfAdd
. . . . . . . . . . . . . ctfcSize
. . . . . . . . . . . . . . ctfc4Bit
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . . . . . . . (IntegerType)ctfc4 = 0
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . . . . . . . (IntegerType)ctfc4 = 1
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . . . . . . . (IntegerType)ctfc4 = 2
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . . . . . . . (IntegerType)ctfc4 = 3
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 11
. . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . UL_DeletedTransChInfoList
. . . . . . . UL_AddReconfTransChInfoList
. . . . . . . . UL_AddReconfTransChInformation
. . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType = 0
. . . . . . . . . (IntegerType)transportChannelIdentity = 1
. . . . . . . . . TransportFormatSet
. . . . . . . . . . DedicatedTransChTFS
. . . . . . . . . . . tti
. . . . . . . . . . . . DedicatedDynamicTF_InfoList
. . . . . . . . . . . . . DedicatedDynamicTF_Info
. . . . . . . . . . . . . . rlc_Size
. . . . . . . . . . . . . . . OctetModeRLC_SizeInfoType1
. . . . . . . . . . . . . . . . (IntegerType)sizeType1 = 16
. . . . . . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . LogicalChannelList
. . . . . . . . . . . SemistaticTF_Information
. . . . . . . . . . . . ChannelCodingType
. . . . . . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . . . . . (IntegerType)rateMatchingAttribute = 155
. . . . . . . . . . . . (CRC_Size)crc_Size = 3
. . . . . . . . UL_AddReconfTransChInformation
. . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType = 0
. . . . . . . . . (IntegerType)transportChannelIdentity = 5
. . . . . . . . . TransportFormatSet
. . . . . . . . . . DedicatedTransChTFS
. . . . . . . . . . . tti
. . . . . . . . . . . . DedicatedDynamicTF_InfoList
. . . . . . . . . . . . . DedicatedDynamicTF_Info
. . . . . . . . . . . . . . rlc_Size
. . . . . . . . . . . . . . . BitModeRLC_SizeInfo
. . . . . . . . . . . . . . . . sizeType2
. . . . . . . . . . . . . . . . . (IntegerType)part1 = 2
. . . . . . . . . . . . . . . . . (IntegerType)part2 = -
. . . . . . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . LogicalChannelList
. . . . . . . . . . . SemistaticTF_Information
. . . . . . . . . . . . ChannelCodingType
. . . . . . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . . . . . (IntegerType)rateMatchingAttribute = 170
. . . . . . . . . . . . (CRC_Size)crc_Size = 3
. . . . . . . modeSpecificTransChInfo
. . . . . . . . fdd
. . . . . . . . . (IntegerType)cpch_SetID = -
. . . . . . . . . DRAC_StaticInformationList
. . . . . . . DL_CommonTransChInfo
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . dl_Parameters
. . . . . . . DL_DeletedTransChInfoList
. . . . . . . DL_AddReconfTransChInfoList
. . . . . . . . DL_AddReconfTransChInformation
. . . . . . . . . (DL_TrCH_Type)dl_TransportChannelType = 0
. . . . . . . . . (IntegerType)dl_transportChannelIdentity = 6
. . . . . . . . . tfs_SignallingMode
. . . . . . . . . . UL_TransportChannelIdentity
. . . . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType = 0
. . . . . . . . . . . (IntegerType)ul_TransportChannelIdentity = 1
. . . . . . . . . QualityTarget
. . . . . . . . . . (IntegerType)bler_QualityValue = -20
. . . . . . . . . TM_SignallingInfo
. . . . . . . . DL_AddReconfTransChInformation
. . . . . . . . . (DL_TrCH_Type)dl_TransportChannelType = 0
. . . . . . . . . (IntegerType)dl_transportChannelIdentity = 10
. . . . . . . . . tfs_SignallingMode
. . . . . . . . . . UL_TransportChannelIdentity
. . . . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType = 0
. . . . . . . . . . . (IntegerType)ul_TransportChannelIdentity = 5
. . . . . . . . . QualityTarget
. . . . . . . . . . (IntegerType)bler_QualityValue = -20
. . . . . . . . . TM_SignallingInfo
. . . . . . . FrequencyInfo
. . . . . . . (IntegerType)maxAllowedUL_TX_Power = 33
. . . . . . . UL_ChannelRequirement
. . . . . . . . UL_DPCH_Info
. . . . . . . . . UL_DPCH_PowerControlInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (IntegerType)dpcch_PowerOffset = -40
. . . . . . . . . . . (IntegerType)pc_Preamble = 1
. . . . . . . . . . . (IntegerType)sRB_delay = 7
. . . . . . . . . . . PowerControlAlgorithm
. . . . . . . . . . . . (IntegerType)algorithm1 = 1
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . (ScramblingCodeType)scramblingCodeType = 1
. . . . . . . . . . . (IntegerType)scramblingCode = 0
. . . . . . . . . . . (IntegerType)numberOfDPDCH = -
. . . . . . . . . . . (SpreadingFactor)spreadingFactor = 4
. . . . . . . . . . . (BooleanType)tfci_Existence = TRUE
. . . . . . . . . . . (IntegerType)numberOfFBI_Bits = -
. . . . . . . . . . . (PuncturingLimit)puncturingLimit = 15
. . . . . . . modeSpecificPhysChInfo
. . . . . . . . fdd
. . . . . . . . . DL_PDSCH_Information
. . . . . . . DL_CommonInformation
. . . . . . . . DL_DPCH_InfoCommon
. . . . . . . . . cfnHandling
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . DL_DPCH_PowerControlInfo
. . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . (DPC_Mode)dpc_Mode = 0
. . . . . . . . . . . (IntegerType)powerOffsetPilot_pdpdch = 0
. . . . . . . . . . . Dl_rate_matching_restriction
. . . . . . . . . . . SF512_AndPilot
. . . . . . . . . . . . (PilotBits128)sfd128 = 0
. . . . . . . . . . . (PositionFixedOrFlexible)positionFixedOrFlexible = 1
. . . . . . . . . . . (BooleanType)tfci_Existence = TRUE
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . (IntegerType)defaultDPCH_OffsetValue = -
. . . . . . . . . . DPCH_CompressedModeInfo
. . . . . . . . . . (TX_DiversityMode)tx_DiversityMode = 0
. . . . . . . . . . SSDT_Information
. . . . . . . DL_InformationPerRL_List
. . . . . . . . DL_InformationPerRL
. . . . . . . . . modeSpecificInfo
. . . . . . . . . . fdd
. . . . . . . . . . . PrimaryCPICH_Info
. . . . . . . . . . . . (IntegerType)primaryScramblingCode = 100
. . . . . . . . . . . PDSCH_SHO_DCH_Info
. . . . . . . . . . . PDSCH_CodeMapping
. . . . . . . . . DL_DPCH_InfoPerRL
. . . . . . . . . . fdd
. . . . . . . . . . . (PCPICH_UsageForChannelEst)pCPICH_UsageForChannelEst = 0
. . . . . . . . . . . (IntegerType)dpch_FrameOffset = 0
. . . . . . . . . . . SecondaryCPICH_Info
. . . . . . . . . . . DL_ChannelisationCodeList
. . . . . . . . . . . . DL_ChannelisationCode
. . . . . . . . . . . . . (IntegerType)secondaryScramblingCode = 1
. . . . . . . . . . . . . SF512_AndCodeNumber
. . . . . . . . . . . . . . (IntegerType)sf128 = 0
. . . . . . . . . . . . . (ScramblingCodeChange)scramblingCodeChange = -
. . . . . . . . . . . (IntegerType)tpc_CombinationIndex = 0
. . . . . . . . . . . (SSDT_CellIdentity)ssdt_CellIdentity = -
. . . . . . . . . . . (ClosedLoopTimingAdjMode)closedLoopTimingAdjMode = -
. . . . . . . . . SCCPCH_InfoForFACH
. . . . . . v3a0NonCriticalExtensions
. . . . . . . RadioBearerSetup_v3a0ext
. . . . . . . . (BitStringType)new_DSCH_RNTI[16] = -
. . . . . . . laterNonCriticalExtensions
- Constraint:
cas_RB_SetUpAM_WithCnf
- BinaryMessage:
30 4f 02 01 ff 02 01 02 02 01 00 80 00 00 00 03 92 04 ba f0 00 00 16 09 b3 1e 96 92 24 95 11 a0 19 c8 56 20 40 38 24 52 49 32 bf 02 00 82 40 22 39 a6 21 00 88 22 3a 96 0c 30 b0 2b 89 89 5d 34 a8 f4 40 00 00 27 c9 00 ac 40 81 90 00 02 0a 00 00

- No.: 2132
- Timestamp: 20:49:01:555_0
- RFN: 3360
- Chip: 7424
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_CNF
- Source: ts_RRC_SetUpRAB_AM_7_RLC LINE 6
- Message Structure:
RLC_AM_DATA_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. (IntegerType)mui = 0
- Constraint:
car_AM_DataMuiCnf
- BinaryMessage:
30 09 02 01 ff 02 01 02 02 01 00

- No.: 2139
- Timestamp: 20:49:01:697_0
- RFN: 3374
- Chip: 16128
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Modify_REQ
- Source: ts_SS_2DCH_Modify LINE 3
- Message Structure:
CPHY_RL_Modify_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
. (RatType)ratType = 0
. CphyRlModifyReq
. . SS_ActivationTime
. . . (IntegerType)activationCFN = 0
. . physicalChannelInfo
. . . DPCHInfo
. . . . UL_DPCH_Info
. . . . DL_DPCHInfo
. . . . . DL_CommonInformation
. . . . . . DL_DPCH_InfoCommon
. . . . . . . cfnHandling
. . . . . . . modeSpecificInfo
. . . . . . . . fdd
. . . . . . . . . DL_DPCH_PowerControlInfo
. . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . fdd
. . . . . . . . . . . . (DPC_Mode)dpc_Mode = 0
. . . . . . . . . (IntegerType)powerOffsetPilot_pdpdch = 0
. . . . . . . . . Dl_rate_matching_restriction
. . . . . . . . . SF512_AndPilot
. . . . . . . . . . (PilotBits128)sfd128 = 0
. . . . . . . . . (PositionFixedOrFlexible)positionFixedOrFlexible = 1
. . . . . . . . . (BooleanType)tfci_Existence = TRUE
. . . . . . modeSpecificInfo
. . . . . . . fdd
. . . . . . . . (IntegerType)defaultDPCH_OffsetValue = -
. . . . . . . . DPCH_CompressedModeInfo
. . . . . . . . (TX_DiversityMode)tx_DiversityMode = 0
. . . . . . . . SSDT_Information
. . . . . DL_DPCH_InfoPerRL
. . . . . . fdd
. . . . . . . (PCPICH_UsageForChannelEst)pCPICH_UsageForChannelEst = 0
. . . . . . . (IntegerType)dpch_FrameOffset = 0
. . . . . . . SecondaryCPICH_Info
. . . . . . . DL_ChannelisationCodeList
. . . . . . . . DL_ChannelisationCode
. . . . . . . . . (IntegerType)secondaryScramblingCode = 1
. . . . . . . . . SF512_AndCodeNumber
. . . . . . . . . . (IntegerType)sf128 = 0
. . . . . . . . . (ScramblingCodeChange)scramblingCodeChange = -
. . . . . . . (IntegerType)tpc_CombinationIndex = 0
. . . . . . . (SSDT_CellIdentity)ssdt_CellIdentity = -
. . . . . . . (ClosedLoopTimingAdjMode)closedLoopTimingAdjMode = -
. . . . . (IntegerType)powerOffsetOfTFCI_PO1 = 0
. . . . . (IntegerType)powerOffsetOfTPC_PO2 = 0
. . . . . (IntegerType)powerOffsetOfPILOT_PO3 = 0
. . . . . (IntegerType)dl_TxPower = -5
. . . . . (IntegerType)dl_TxPowerMax = 15
. . . . . (IntegerType)dl_TxPowerMin = -35
- Constraint:
ca_DL_DPCH_ModifyInfo
- BinaryMessage:
30 5d 02 01 00 02 01 1a 0a 01 00 30 52 02 01 00 30 4d 30 4b 30 21 30 19 05 00 30 30 14 30 06 30 30 03 0a 01 00 02 01 00 0a 01 00 0a 01 01 01 01 ff 30 30 03 0a 01 00 30 30 13 0a 01 00 02 01 00 30 08 30 06 02 01 01 02 01 00 02 01 00 02 01 00 02 01 00 02 01 00 02 01 fb 02 01 0f 02 01 dd

- No.: 2143
- Timestamp: 20:49:01:753_0
- RFN: 3380
- Chip: 1792
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Modify_CNF
- Source: ts_SS_2DCH_Modify LINE 4
- Message Structure:
CPHY_RL_Modify_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
ca_RL_ModifyCnf
- BinaryMessage:
30 06 02 01 00 02 01 1a

- No.: 2144
- Timestamp: 20:49:01:785_0
- RFN: 3383
- Chip: 7936
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Config_REQ
- Source: ts_SS_2DCH_Modify LINE 5
- Message Structure:
CPHY_TrCH_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
. (RatType)ratType = 0
. CphyTrchConfigReq
. . SS_ActivationTime
. . . (IntegerType)activationCFN = 0
. . ulconnectedTrCHList
. . TFCS
. . dlconnectedTrCHList
. . . CphyTrchConfigReq_setseq_1
. . . . (IntegerType)trchid = 6
. . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 144
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional = 1
. . . . . . (IntegerType)rateMatchingAttribute = 155
. . . . . . (CRC_Size)crc_Size = 3
. . . CphyTrchConfigReq_setseq_1
. . . . (IntegerType)trchid = 10
. . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 148
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional = 1
. . . . . . (IntegerType)rateMatchingAttribute = 170
. . . . . . (CRC_Size)crc_Size = 3
. . TFCS
. . . ExplicitTFCS_Configuration
. . . . TFCS_ReconfAdd
. . . . . ctfcSize
. . . . . . ctfc4Bit
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 0
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 1
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 2
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 3
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . fdd
. . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 9
. . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m = -
- Constraint:
ca_TrChCfgInfo
- BinaryMessage:
30 81 95 02 01 00 02 01 1a 0a 01 00 30 81 89 02 01 00 30 4c 30 24 02 01 06 0a 01 00 30 1c 30 0e 30 0c 02 02 00 90 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 9b 0a 01 03 30 24 02 01 0a 0a 01 00 30 1c 30 0e 30 0c 02 02 00 94 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 aa 0a 01 03 30 36 30 30 33 30 08 02 01 00 30 03 02 01 00 30 08 02 01 01 30 03 02 01 00 30 08 02 01 02 30 03 02 01 00 30 13 02 01 03 30 0e 30 0c 30 30 03 02 01 09 02 01 0f 02 01 00

- No.: 2148
- Timestamp: 20:49:01:837_0
- RFN: 3388
- Chip: 16640
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Config_CNF
- Source: ts_SS_2DCH_Modify LINE 6
- Message Structure:
CPHY_TrCH_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
ca_TrChCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 1a

- No.: 2149
- Timestamp: 20:49:01:896_0
- RFN: 3394
- Chip: 13056
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_SS_2DCH_Modify LINE 7
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
. (RatType)ratType = 0
. configMessage
. . CmacConfigReq
. . . SS_ActivationTime
. . . . (IntegerType)activationCFN = 0
. . . UE_Info
. . . . U_RNTI
. . . . (BitStringType)c_RNTI[16] = -
. . . TrCHInfo
. . . . ulconnectedTrCHList
. . . . TFCS
. . . . dlconnectedTrCHList
. . . . . TrCHInfo_setseq_1
. . . . . . (IntegerType)trchid = 6
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 144
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . (IntegerType)rateMatchingAttribute = 155
. . . . . . . . (CRC_Size)crc_Size = 3
. . . . . TrCHInfo_setseq_1
. . . . . . (IntegerType)trchid = 10
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 148
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . (IntegerType)rateMatchingAttribute = 170
. . . . . . . . (CRC_Size)crc_Size = 3
. . . . TFCS
. . . . . ExplicitTFCS_Configuration
. . . . . . TFCS_ReconfAdd
. . . . . . . ctfcSize
. . . . . . . . ctfc4Bit
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 0
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 1
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 2
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 3
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC = 9
. . . . . . . . . . . . . (IntegerType)gainFactorBetaD = 15
. . . . . . . . . . . . . (IntegerType)referenceTFC_ID = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m = -
. . . TrCH_LogCHMappingList1
. . . . ulconnectedTrCHList
. . . . dlconnectedTrCHList
. . . . . TrCH_LogCHMappingList1_setseq_1
. . . . . . (IntegerType)trchid = 6
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 7
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 5
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 7
. . . . . . . . (IntegerType)rB_Identity = -12
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . TrCH_LogCHMappingList1_setseq_1
. . . . . . (IntegerType)trchid = 10
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 1
. . . . . . . . (IntegerType)rB_Identity = 1
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 2
. . . . . . . . (IntegerType)rB_Identity = 2
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 3
. . . . . . . . (IntegerType)rB_Identity = 3
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority = 4
. . . . . . . . (IntegerType)rB_Identity = 4
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_CMAC_ReconfigInfo
- BinaryMessage:
30 82 01 21 02 01 ff 02 01 1a 0a 01 00 30 82 01 14 02 01 00 30 00 30 81 80 30 46 30 21 02 01 06 30 1c 30 0e 30 0c 02 02 00 90 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 9b 0a 01 03 30 21 02 01 0a 30 1c 30 0e 30 0c 02 02 00 94 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 aa 0a 01 03 30 36 30 30 33 30 08 02 01 00 30 03 02 01 00 30 08 02 01 01 30 03 02 01 00 30 08 02 01 02 30 03 02 01 00 30 13 02 01 03 30 0e 30 0c 30 30 03 02 01 09 02 01 0f 02 01 00 30 81 89 30 81 86 30 1d 02 01 06 30 18 30 16 30 11 0a 01 00 0a 01 00 02 01 07 0a 01 05 05 00 02 01 07 02 01 f4 30 65 02 01 0a 30 60 30 16 30 11 0a 01 00 0a 01 00 02 01 01 0a 01 04 05 00 02 01 01 02 01 01 30 16 30 11 0a 01 00 0a 01 00 02 01 02 0a 01 04 05 00 02 01 02 02 01 02 30 16 30 11 0a 01 00 0a 01 00 02 01 03 0a 01 04 05 00 02 01 03 02 01 03 30 16 30 11 0a 01 00 0a 01 00 02 01 04 0a 01 04 05 00 02 01 04 02 01 04

- No.: 2150
- Timestamp: 20:49:01:932_0
- RFN: 3397
- Chip: 36096
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_SS_2DCH_Modify LINE 8
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 1a

- No.: 2151
- Timestamp: 20:49:01:962_0
- RFN: 3400
- Chip: 35840
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Modify_REQ
- Source: ts_SS_2DCH_Modify LINE 9
- Message Structure:
CPHY_RL_Modify_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
. (RatType)ratType = 0
. CphyRlModifyReq
. . SS_ActivationTime
. . . (IntegerType)activationCFN = 0
. . physicalChannelInfo
. . . DPCHInfo
. . . . UL_DPCH_Info
. . . . . UL_DPCH_PowerControlInfo
. . . . . . fdd
. . . . . . . (IntegerType)dpcch_PowerOffset = -40
. . . . . . . (IntegerType)pc_Preamble = 1
. . . . . . . (IntegerType)sRB_delay = 7
. . . . . . . PowerControlAlgorithm
. . . . . . . . (IntegerType)algorithm1 = 1
. . . . . modeSpecificInfo
. . . . . . fdd
. . . . . . . (ScramblingCodeType)scramblingCodeType = 1
. . . . . . . (IntegerType)scramblingCode = 0
. . . . . . . (IntegerType)numberOfDPDCH = -
. . . . . . . (SpreadingFactor)spreadingFactor = 4
. . . . . . . (BooleanType)tfci_Existence = TRUE
. . . . . . . (IntegerType)numberOfFBI_Bits = -
. . . . . . . (PuncturingLimit)puncturingLimit = 15
. . . . DL_DPCHInfo
- Constraint:
ca_UL_DPCH_ModifyInfo
- BinaryMessage:
30 33 02 01 00 02 01 14 0a 01 00 30 28 02 01 00 30 23 30 21 30 30 0c 02 01 d8 02 01 01 02 01 07 02 01 01 30 30 0f 0a 01 01 02 01 00 0a 01 04 01 01 ff 0a 01 0f

- No.: 2155
- Timestamp: 20:49:02:012_0
- RFN: 3405
- Chip: 36864
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Modify_CNF
- Source: ts_SS_2DCH_Modify LINE 10
- Message Structure:
CPHY_RL_Modify_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_RL_ModifyCnf
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 2156
- Timestamp: 20:49:02:038_0
- RFN: 3408
- Chip: 22528
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Config_REQ
- Source: ts_SS_2DCH_Modify LINE 11
- Message Structure:
CPHY_TrCH_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
. (RatType)ratType = 0
. CphyTrchConfigReq
. . SS_ActivationTime
. . . (IntegerType)activationCFN = 0
. . ulconnectedTrCHList
. . . CphyTrchConfigReq_setseq_0
. . . . (IntegerType)trchid = 1
. . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 144
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional = 1
. . . . . . (IntegerType)rateMatchingAttribute = 155
. . . . . . (CRC_Size)crc_Size = 3
. . . CphyTrchConfigReq_setseq_0
. . . . (IntegerType)trchid = 5
. . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size = 148
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional = 1
. . . . . . (IntegerType)rateMatchingAttribute = 170
. . . . . . (CRC_Size)crc_Size = 3
. . TFCS
. . . ExplicitTFCS_Configuration
. . . . TFCS_ReconfAdd
. . . . . ctfcSize
. . . . . . ctfc4Bit
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 0
. . . . . . . . PowerOffsetInformation
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 1
. . . . . . . . PowerOffsetInformation
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 2
. . . . . . . . PowerOffsetInformation
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4 = 3
. . . . . . . . PowerOffsetInformation
. . dlconnectedTrCHList
. . TFCS
- Constraint:
ca_TrChCfgInfo
- BinaryMessage:
30 75 02 01 00 02 01 14 0a 01 00 30 6a 02 01 00 30 4c 30 24 02 01 01 0a 01 00 30 1c 30 0e 30 0c 02 02 00 90 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 9b 0a 01 03 30 24 02 01 05 0a 01 00 30 1c 30 0e 30 0c 02 02 00 94 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 aa 0a 01 03 30 17 30 30 14 30 03 02 01 00 30 03 02 01 01 30 03 02 01 02 30 03 02 01 03

- No.: 2160
- Timestamp: 20:49:02:087_0
- RFN: 3413
- Chip: 14592
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Config_CNF
- Source: ts_SS_2DCH_Modify LINE 12
- Message Structure:
CPHY_TrCH_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_TrChCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 2161
- Timestamp: 20:49:02:150_0
- RFN: 3419
- Chip: 28928
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_SS_2DCH_Modify LINE 13
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
. (RatType)ratType = 0
. configMessage
. . CmacConfigReq
. . . SS_ActivationTime
. . . . (IntegerType)activationCFN = 0
. . . UE_Info
. . . . U_RNTI
. . . . (BitStringType)c_RNTI[16] = -
. . . TrCHInfo
. . . . ulconnectedTrCHList
. . . . . TrCHInfo_setseq_0
. . . . . . (IntegerType)trchid = 1
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 144
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . (IntegerType)rateMatchingAttribute = 155
. . . . . . . . (CRC_Size)crc_Size = 3
. . . . . TrCHInfo_setseq_0
. . . . . . (IntegerType)trchid = 5
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size = 148
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional = 1
. . . . . . . . (IntegerType)rateMatchingAttribute = 170
. . . . . . . . (CRC_Size)crc_Size = 3
. . . . TFCS
. . . . . ExplicitTFCS_Configuration
. . . . . . TFCS_ReconfAdd
. . . . . . . ctfcSize
. . . . . . . . ctfc4Bit
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 0
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 1
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 2
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4 = 3
. . . . . . . . . . PowerOffsetInformation
. . . . dlconnectedTrCHList
. . . . TFCS
. . . TrCH_LogCHMappingList1
. . . . ulconnectedTrCHList
. . . . . TrCH_LogCHMappingList1_setseq_0
. . . . . . (IntegerType)trchid = 1
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 7
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 5
. . . . . . . . (IntegerType)rB_Identity = -12
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . TrCH_LogCHMappingList1_setseq_0
. . . . . . (IntegerType)trchid = 5
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 1
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . (IntegerType)rB_Identity = 1
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 2
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . (IntegerType)rB_Identity = 2
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 3
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . (IntegerType)rB_Identity = 3
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType = 0
. . . . . . . . . . (IntegerType)logicalChannelIdentity = 4
. . . . . . . . . . (LogicalChannelType)logicalChannelType = 4
. . . . . . . . (IntegerType)rB_Identity = 4
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity = -
. . . . dlconnectedTrCHList
- Constraint:
ca_CMAC_ReconfigInfo
- BinaryMessage:
30 81 e5 02 01 ff 02 01 14 0a 01 00 30 81 d9 02 01 00 30 00 30 61 30 46 30 21 02 01 01 30 1c 30 0e 30 0c 02 02 00 90 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 9b 0a 01 03 30 21 02 01 05 30 1c 30 0e 30 0c 02 02 00 94 30 04 05 00 05 00 05 00 30 0a 0a 01 01 02 02 00 aa 0a 01 03 30 17 30 30 14 30 03 02 01 00 30 03 02 01 01 30 03 02 01 02 30 03 02 01 03 30 6f 30 6d 30 18 02 01 01 30 13 30 11 30 0c 0a 01 00 0a 01 00 02 01 07 0a 01 05 02 01 f4 30 51 02 01 05 30 4c 30 11 30 0c 0a 01 00 0a 01 00 02 01 01 0a 01 04 02 01 01 30 11 30 0c 0a 01 00 0a 01 00 02 01 02 0a 01 04 02 01 02 30 11 30 0c 0a 01 00 0a 01 00 02 01 03 0a 01 04 02 01 03 30 11 30 0c 0a 01 00 0a 01 00 02 01 04 0a 01 04 02 01 04

- No.: 2162
- Timestamp: 20:49:02:184_0
- RFN: 3423
- Chip: 5376
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_SS_2DCH_Modify LINE 14
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 14

- No.: 2165
- Timestamp: 20:49:02:195_0
- RFN: 3424
- Chip: 8960
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB_TM_Cfg_RLC LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = -12
. (RatType)ratType = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_TM_RLC_Mode
. . . . . . (BooleanType)segmentationIndication = TRUE
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize = 144
. . . . . UL_RLC_Mode
. . . . . . UL_TM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . (BooleanType)segmentationIndication = TRUE
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity = 7
. . . . (IntegerType)dLlogicalChannelIdentity = 7
. . . . (LogicalChannelType)logicalChannelType = -
. . . . (CN_DomainIdentity)cn_DomainIdentity = -
- Constraint:
ca_RB_TM_Info
- BinaryMessage:
30 25 02 01 ff 02 01 f4 0a 01 00 30 1a 30 10 30 03 01 01 ff 30 09 02 02 00 90 30 03 01 01 ff 30 06 02 01 07 02 01 07

- No.: 2169
- Timestamp: 20:49:02:208_0
- RFN: 3425
- Chip: 18944
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB_TM_Cfg_RLC LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = -12
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 f4

- No.: 2177
- Timestamp: 20:49:02:216_1
- RFN: 3426
- Chip: 13312
- Event: Start Timer
- Source: ts_RRC_ReceiveRB_SetupCmpl LINE 2
- Message Structure:
no details available
- Constraint:
t_WaitMS (13500 Ms)
- BinaryMessage:

- No.: 2186
- Timestamp: 20:49:03:901_0
- RFN: 3594
- Chip: 33280
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_IND
- Source: ts_RRC_ReceiveRB_SetupCmpl:lt_CipheringNotStartedAM_RAB LINE 4
- Message Structure:
RLC_AM_DATA_IND
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. IntegrityResult
. . (IntegrityStatus)integrityUsed = 0
. aM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "11011110110000110001011001100110"
. . . . (IntegerType)rrc_MessageSequenceNumber = 4
. . . UL_DCCH_MessageType
. . . . RadioBearerSetupComplete
. . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . IntegrityProtActivationInfo
. . . . . (IntegerType)ul_TimingAdvance = 0
. . . . . (BitStringType)start_Value[20] = "00000000000000000100"
. . . . . (IntegerType)count_C_ActivationTime = 0
. . . . . UL_CounterSynchronisationInfo
. . . . . laterNonCriticalExtensions
. . . . . . (BitStringType)radioBearerSetupComplete_r3_add_ext = 0
. . . . . . nonCriticalExtensions
- Constraint:
car_RB_SetUpCmpl
- BinaryMessage:
30 12 02 01 ff 02 01 02 0a 01 00 ef 61 8b 33 23 c8 00 00 08

- No.: 2187
- Timestamp: 20:49:03:902_0
- RFN: 3595
- Chip: 0
- Event: Cancel Timer
- Source: ts_RRC_ReceiveRB_SetupCmpl:lt_CipheringNotStartedAM_RAB LINE 4
- Message Structure:
no details available
- Constraint:
t_WaitMS
- BinaryMessage:

- No.: 2188
- Timestamp: 20:49:03:903_0
- RFN: 3595
- Chip: 1024
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ReceiveRB_SetupCmpl:lt_CipheringNotStartedAM_RAB LINE 4
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2213
- Timestamp: 20:49:03:939_0
- RFN: 3598
- Chip: 26624
- Event: Send
- PCO: Dc
- Message: RRC_DataReq
- Source: ts_TC_CloseUE_TestLoop LINE 6
- Message Structure:
RRC_DataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[-1] = -
. (SapId)sapId[1] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. CLOSEUETESTLOOP
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)tCProtocolDiscriminator[4] = '1111'B
. . (MsgType)msgType[8] = '01000000'B
. . (UE_TestLoopMode)uE_TestLoopMode[1] = '00'O
. . UE_TestLoopMode1LB_Setup
. . . (Length)iel[1] = '03'O
. . . LB_SetupRB_IE
. . . . (BitStringType)rLC_SDU_Size[16] = '0000000011111000'B
. . . . (BitStringType)spare_2[3] = '000'B
. . . . (BitStringType)rB_Identity[5] = '10100'B
. . . LB_SetupRB_IE
. . . LB_SetupRB_IE
. . . LB_SetupRB_IE
- Constraint:
ca_PS_DataReq
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 0f 40 00 03 00 f8 14

- No.: 2214
- Timestamp: 20:49:03:941_0
- RFN: 3598
- Chip: 32000
- Event: Start Timer
- Source: ts_TC_CloseUE_TestLoop LINE 6
- Message Structure:
no details available
- Constraint:
t_Dly (5000 Ms)
- BinaryMessage:

- No.: 2218
- Timestamp: 20:49:04:216_0
- RFN: 3626
- Chip: 13824
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_TC_CloseUE_TestLoop LINE 7
- Message Structure:
RRC_DataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. (START_Value)start[0] = -
. CLOSEUETESTLOOPCOMPLETE
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)tCProtocolDiscriminator[4] = '1111'B
. . (MsgType)msgType[8] = '01000001'B
- Constraint:
car_PS_UplinkDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 0f 41

- No.: 2219
- Timestamp: 20:49:04:217_0
- RFN: 3626
- Chip: 17152
- Event: Cancel Timer
- Source: ts_TC_CloseUE_TestLoop LINE 7
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 2220
- Timestamp: 20:49:04:217_1
- RFN: 3626
- Chip: 18176
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_TC_CloseUE_TestLoop LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2227
- Timestamp: 20:49:04:228_1
- RFN: 3627
- Chip: 23040
- Event: Start Timer
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 5
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 2234
- Timestamp: 20:49:04:254_0
- RFN: 3630
- Chip: 5632
- Event: Timeout
- Source: tc_7_2_3_18:lt_TxAndRx LINE 5
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 2254
- Timestamp: 20:49:04:292_0
- RFN: 3633
- Chip: 33024
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000000'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'FFE665A5C5CA3452085408ABEECE4B'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 01 1e ff e6 65 a5 c5 ca 34 52 08 54 08 ab ee ce 4b

- No.: 2263
- Timestamp: 20:49:04:305_0
- RFN: 3635
- Chip: 6144
- Event: Start Timer
- Source: tc_7_2_3_18:lt_TxAndRx LINE 9
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 2264
- Timestamp: 20:49:04:305_1
- RFN: 3635
- Chip: 7424
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2269
- Timestamp: 20:49:04:322_1
- RFN: 3636
- Chip: 34048
- Event: Timeout
- Source: tc_7_2_3_18:lt_TxAndRx LINE 5
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 2289
- Timestamp: 20:49:04:360_0
- RFN: 3640
- Chip: 27904
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000001'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '0B813FD337873F2CD1E29AE91BD6C8'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 09 1e 0b 81 3f d3 37 87 3f 2c d1 e2 9a e9 1b d6 c8

- No.: 2298
- Timestamp: 20:49:04:374_0
- RFN: 3642
- Chip: 3328
- Event: Start Timer
- Source: tc_7_2_3_18:lt_TxAndRx LINE 9
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 2299
- Timestamp: 20:49:04:374_1
- RFN: 3642
- Chip: 4096
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2304
- Timestamp: 20:49:04:389_0
- RFN: 3643
- Chip: 22528
- Event: Timeout
- Source: tc_7_2_3_18:lt_TxAndRx LINE 5
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 2324
- Timestamp: 20:49:04:427_0
- RFN: 3647
- Chip: 17152
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000010'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'E14FDE630F8195688EBE465F09816A'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 11 1e e1 4f de 63 0f 81 95 68 8e be 46 5f 09 81 6a

- No.: 2333
- Timestamp: 20:49:04:443_0
- RFN: 3649
- Chip: 256
- Event: Start Timer
- Source: tc_7_2_3_18:lt_TxAndRx LINE 9
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 2334
- Timestamp: 20:49:04:443_1
- RFN: 3649
- Chip: 1024
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2337
- Timestamp: 20:49:04:454_0
- RFN: 3650
- Chip: 3840
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_18:lt_TxAndRx LINE 3
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000000'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . (AM_Data)data[16] = 'FFE665A5C5CA3452085408ABEECE4BFF'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 00 ff e6 65 a5 c5 ca 34 52 08 54 08 ab ee ce 4b ff

- No.: 2348
- Timestamp: 20:49:04:467_1
- RFN: 3651
- Chip: 17664
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2351
- Timestamp: 20:49:04:474_0
- RFN: 3652
- Chip: 4608
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_18:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000001'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = 'E665A5C5CA3452085408ABEECE4BFF'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 09 1e e6 65 a5 c5 ca 34 52 08 54 08 ab ee ce 4b ff

- No.: 2362
- Timestamp: 20:49:04:487_1
- RFN: 3653
- Chip: 16896
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2365
- Timestamp: 20:49:04:490_1
- RFN: 3653
- Chip: 29440
- Event: Timeout
- Source: tc_7_2_3_18:lt_TxAndRx LINE 5
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 2385
- Timestamp: 20:49:04:534_0
- RFN: 3658
- Chip: 4608
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000011'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '8EEB1B83953DD362DAE3B06D5B76D8'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 19 1e 8e eb 1b 83 95 3d d3 62 da e3 b0 6d 5b 76 d8

- No.: 2394
- Timestamp: 20:49:04:547_0
- RFN: 3659
- Chip: 17152
- Event: Start Timer
- Source: tc_7_2_3_18:lt_TxAndRx LINE 9
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 2395
- Timestamp: 20:49:04:547_1
- RFN: 3659
- Chip: 18176
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2398
- Timestamp: 20:49:04:555_0
- RFN: 3660
- Chip: 12032
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_18:lt_TxAndRx LINE 3
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000010'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . (AM_Data)data[16] = '0B813FD337873F2CD1E29AE91BD6C80B'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 10 0b 81 3f d3 37 87 3f 2c d1 e2 9a e9 1b d6 c8 0b

- No.: 2409
- Timestamp: 20:49:04:569_2
- RFN: 3661
- Chip: 26368
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2412
- Timestamp: 20:49:04:577_0
- RFN: 3662
- Chip: 20224
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_18:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000011'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '813FD337873F2CD1E29AE91BD6C80B'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 19 1e 81 3f d3 37 87 3f 2c d1 e2 9a e9 1b d6 c8 0b

- No.: 2423
- Timestamp: 20:49:04:595_0
- RFN: 3664
- Chip: 5632
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2426
- Timestamp: 20:49:04:603_0
- RFN: 3664
- Chip: 37376
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_18:lt_TxAndRx LINE 3
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000100'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . (AM_Data)data[16] = 'E14FDE630F8195688EBE465F09816AE1'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 20 e1 4f de 63 0f 81 95 68 8e be 46 5f 09 81 6a e1

- No.: 2437
- Timestamp: 20:49:04:616_1
- RFN: 3666
- Chip: 11776
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2440
- Timestamp: 20:49:04:623_0
- RFN: 3666
- Chip: 37376
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_18:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000101'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '4FDE630F8195688EBE465F09816AE1'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 29 1e 4f de 63 0f 81 95 68 8e be 46 5f 09 81 6a e1

- No.: 2451
- Timestamp: 20:49:04:636_2
- RFN: 3668
- Chip: 12800
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2454
- Timestamp: 20:49:04:640_1
- RFN: 3668
- Chip: 26112
- Event: Timeout
- Source: tc_7_2_3_18:lt_TxAndRx LINE 5
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 2474
- Timestamp: 20:49:04:679_0
- RFN: 3672
- Chip: 22272
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000100'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'E3E53087EA645A09017FD99C3CACBB'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 21 1e e3 e5 30 87 ea 64 5a 09 01 7f d9 9c 3c ac bb

- No.: 2483
- Timestamp: 20:49:04:695_1
- RFN: 3674
- Chip: 8704
- Event: Start Timer
- Source: tc_7_2_3_18:lt_TxAndRx LINE 9
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 2484
- Timestamp: 20:49:04:695_2
- RFN: 3674
- Chip: 9472
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2487
- Timestamp: 20:49:04:704_0
- RFN: 3675
- Chip: 3584
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_18:lt_TxAndRx LINE 3
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000110'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . (AM_Data)data[16] = '8EEB1B83953DD362DAE3B06D5B76D88E'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 30 8e eb 1b 83 95 3d d3 62 da e3 b0 6d 5b 76 d8 8e

- No.: 2498
- Timestamp: 20:49:04:720_0
- RFN: 3676
- Chip: 26368
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2501
- Timestamp: 20:49:04:726_0
- RFN: 3677
- Chip: 13312
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_18:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000111'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = 'EB1B83953DD362DAE3B06D5B76D88E'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 39 1e eb 1b 83 95 3d d3 62 da e3 b0 6d 5b 76 d8 8e

- No.: 2512
- Timestamp: 20:49:04:739_2
- RFN: 3678
- Chip: 25344
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2515
- Timestamp: 20:49:04:743_1
- RFN: 3679
- Chip: 768
- Event: Timeout
- Source: tc_7_2_3_18:lt_TxAndRx LINE 5
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 2535
- Timestamp: 20:49:04:782_0
- RFN: 3682
- Chip: 36352
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000101'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '46DF1CD61DA9C435F89943DF9CC34A'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 29 1e 46 df 1c d6 1d a9 c4 35 f8 99 43 df 9c c3 4a

- No.: 2544
- Timestamp: 20:49:04:795_0
- RFN: 3684
- Chip: 9472
- Event: Start Timer
- Source: tc_7_2_3_18:lt_TxAndRx LINE 9
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 2545
- Timestamp: 20:49:04:795_1
- RFN: 3684
- Chip: 10240
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2550
- Timestamp: 20:49:04:812_1
- RFN: 3685
- Chip: 36096
- Event: Timeout
- Source: tc_7_2_3_18:lt_TxAndRx LINE 5
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 2570
- Timestamp: 20:49:04:856_0
- RFN: 3690
- Chip: 13568
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000110'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'DEE31AD6E24FA1903D53778D949742'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 31 1e de e3 1a d6 e2 4f a1 90 3d 53 77 8d 94 97 42

- No.: 2579
- Timestamp: 20:49:04:869_1
- RFN: 3691
- Chip: 25856
- Event: Start Timer
- Source: tc_7_2_3_18:lt_TxAndRx LINE 9
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 2580
- Timestamp: 20:49:04:869_2
- RFN: 3691
- Chip: 26880
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2583
- Timestamp: 20:49:04:878_0
- RFN: 3692
- Chip: 20480
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_18:lt_TxAndRx LINE 3
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000001000'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . (AM_Data)data[16] = 'E3E53087EA645A09017FD99C3CACBBE3'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 40 e3 e5 30 87 ea 64 5a 09 01 7f d9 9c 3c ac bb e3

- No.: 2594
- Timestamp: 20:49:04:892_1
- RFN: 3693
- Chip: 33536
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2597
- Timestamp: 20:49:04:899_0
- RFN: 3694
- Chip: 20992
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_18:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000001001'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = 'E53087EA645A09017FD99C3CACBBE3'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 49 1e e5 30 87 ea 64 5a 09 01 7f d9 9c 3c ac bb e3

- No.: 2608
- Timestamp: 20:49:04:912_1
- RFN: 3695
- Chip: 34048
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2611
- Timestamp: 20:49:04:915_1
- RFN: 3696
- Chip: 8448
- Event: Timeout
- Source: tc_7_2_3_18:lt_TxAndRx LINE 5
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 2631
- Timestamp: 20:49:04:959_0
- RFN: 3700
- Chip: 24576
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000000111'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '750DD49DE9CE9E430AD448A14575D8'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 39 1e 75 0d d4 9d e9 ce 9e 43 0a d4 48 a1 45 75 d8

- No.: 2640
- Timestamp: 20:49:04:973_0
- RFN: 3701
- Chip: 37888
- Event: Start Timer
- Source: tc_7_2_3_18:lt_TxAndRx LINE 9
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 2641
- Timestamp: 20:49:04:973_1
- RFN: 3702
- Chip: 256
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2644
- Timestamp: 20:49:04:981_0
- RFN: 3702
- Chip: 32000
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_18:lt_TxAndRx LINE 3
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000001010'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . (AM_Data)data[16] = '46DF1CD61DA9C435F89943DF9CC34A46'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 50 46 df 1c d6 1d a9 c4 35 f8 99 43 df 9c c3 4a 46

- No.: 2655
- Timestamp: 20:49:04:995_1
- RFN: 3704
- Chip: 8448
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2658
- Timestamp: 20:49:05:001_0
- RFN: 3704
- Chip: 33024
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_18:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000001011'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = 'DF1CD61DA9C435F89943DF9CC34A46'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 59 1e df 1c d6 1d a9 c4 35 f8 99 43 df 9c c3 4a 46

- No.: 2669
- Timestamp: 20:49:05:018_1
- RFN: 3706
- Chip: 18688
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2672
- Timestamp: 20:49:05:026_0
- RFN: 3707
- Chip: 12800
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_18:lt_TxAndRx LINE 3
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000001100'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . (AM_Data)data[16] = 'DEE31AD6E24FA1903D53778D949742DE'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 60 de e3 1a d6 e2 4f a1 90 3d 53 77 8d 94 97 42 de

- No.: 2683
- Timestamp: 20:49:05:042_1
- RFN: 3708
- Chip: 34560
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2686
- Timestamp: 20:49:05:048_0
- RFN: 3709
- Chip: 22272
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_18:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000001101'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = 'E31AD6E24FA1903D53778D949742DE'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 69 1e e3 1a d6 e2 4f a1 90 3d 53 77 8d 94 97 42 de

- No.: 2697
- Timestamp: 20:49:05:062_1
- RFN: 3710
- Chip: 35072
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2700
- Timestamp: 20:49:05:065_1
- RFN: 3711
- Chip: 10496
- Event: Timeout
- Source: tc_7_2_3_18:lt_TxAndRx LINE 5
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 2720
- Timestamp: 20:49:05:104_0
- RFN: 3715
- Chip: 6400
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000001000'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '9C160255088140200555DDC9CBCB9E'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 41 1e 9c 16 02 55 08 81 40 20 05 55 dd c9 cb cb 9e

- No.: 2729
- Timestamp: 20:49:05:120_0
- RFN: 3716
- Chip: 28416
- Event: Start Timer
- Source: tc_7_2_3_18:lt_TxAndRx LINE 9
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 2730
- Timestamp: 20:49:05:120_1
- RFN: 3716
- Chip: 29440
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2733
- Timestamp: 20:49:05:131_0
- RFN: 3717
- Chip: 32000
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_18:lt_TxAndRx LINE 3
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000001110'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . (AM_Data)data[16] = '750DD49DE9CE9E430AD448A14575D875'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 70 75 0d d4 9d e9 ce 9e 43 0a d4 48 a1 45 75 d8 75

- No.: 2744
- Timestamp: 20:49:05:144_2
- RFN: 3719
- Chip: 7424
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2747
- Timestamp: 20:49:05:151_0
- RFN: 3719
- Chip: 33024
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_18:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000001111'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '0DD49DE9CE9E430AD448A14575D875'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 79 1e 0d d4 9d e9 ce 9e 43 0a d4 48 a1 45 75 d8 75

- No.: 2758
- Timestamp: 20:49:05:164_2
- RFN: 3721
- Chip: 7168
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2761
- Timestamp: 20:49:05:168_0
- RFN: 3721
- Chip: 19968
- Event: Timeout
- Source: tc_7_2_3_18:lt_TxAndRx LINE 5
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 2781
- Timestamp: 20:49:05:208_0
- RFN: 3725
- Chip: 18176
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000001001'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'C31F833F866A5BA390680EAB11282E'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 49 1e c3 1f 83 3f 86 6a 5b a3 90 68 0e ab 11 28 2e

- No.: 2790
- Timestamp: 20:49:05:221_1
- RFN: 3726
- Chip: 30464
- Event: Start Timer
- Source: tc_7_2_3_18:lt_TxAndRx LINE 9
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 2791
- Timestamp: 20:49:05:221_2
- RFN: 3726
- Chip: 31488
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2796
- Timestamp: 20:49:05:238_1
- RFN: 3728
- Chip: 18176
- Event: Timeout
- Source: tc_7_2_3_18:lt_TxAndRx LINE 5
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 2816
- Timestamp: 20:49:05:282_0
- RFN: 3732
- Chip: 34048
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000001010'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'AE44F5E7658F6B247A0C54A21057F7'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 51 1e ae 44 f5 e7 65 8f 6b 24 7a 0c 54 a2 10 57 f7

- No.: 2825
- Timestamp: 20:49:05:295_0
- RFN: 3734
- Chip: 7936
- Event: Start Timer
- Source: tc_7_2_3_18:lt_TxAndRx LINE 9
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 2826
- Timestamp: 20:49:05:295_1
- RFN: 3734
- Chip: 8960
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2829
- Timestamp: 20:49:05:303_0
- RFN: 3735
- Chip: 2048
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_18:lt_TxAndRx LINE 3
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000010000'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . (AM_Data)data[16] = '9C160255088140200555DDC9CBCB9E9C'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 80 9c 16 02 55 08 81 40 20 05 55 dd c9 cb cb 9e 9c

- No.: 2840
- Timestamp: 20:49:05:317_1
- RFN: 3736
- Chip: 15872
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2843
- Timestamp: 20:49:05:324_0
- RFN: 3737
- Chip: 4352
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_18:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000010001'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '160255088140200555DDC9CBCB9E9C'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 89 1e 16 02 55 08 81 40 20 05 55 dd c9 cb cb 9e 9c

- No.: 2854
- Timestamp: 20:49:05:337_2
- RFN: 3738
- Chip: 17408
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2857
- Timestamp: 20:49:05:341_0
- RFN: 3738
- Chip: 30208
- Event: Timeout
- Source: tc_7_2_3_18:lt_TxAndRx LINE 5
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 2877
- Timestamp: 20:49:05:384_0
- RFN: 3743
- Chip: 5376
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000001011'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '3278595C235077F267A59097E8CEB4'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 59 1e 32 78 59 5c 23 50 77 f2 67 a5 90 97 e8 ce b4

- No.: 2886
- Timestamp: 20:49:05:396_0
- RFN: 3744
- Chip: 12032
- Event: Start Timer
- Source: tc_7_2_3_18:lt_TxAndRx LINE 9
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 2887
- Timestamp: 20:49:05:396_1
- RFN: 3744
- Chip: 12800
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2890
- Timestamp: 20:49:05:403_0
- RFN: 3745
- Chip: 2304
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_18:lt_TxAndRx LINE 3
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000010010'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . (AM_Data)data[16] = 'C31F833F866A5BA390680EAB11282EC3'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 90 c3 1f 83 3f 86 6a 5b a3 90 68 0e ab 11 28 2e c3

- No.: 2901
- Timestamp: 20:49:05:417_0
- RFN: 3746
- Chip: 15360
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2904
- Timestamp: 20:49:05:423_0
- RFN: 3747
- Chip: 2560
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_18:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000010011'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '1F833F866A5BA390680EAB11282EC3'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 99 1e 1f 83 3f 86 6a 5b a3 90 68 0e ab 11 28 2e c3

- No.: 2915
- Timestamp: 20:49:05:439_2
- RFN: 3748
- Chip: 25088
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2918
- Timestamp: 20:49:05:447_0
- RFN: 3749
- Chip: 18944
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_18:lt_TxAndRx LINE 3
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000010100'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . (AM_Data)data[16] = 'AE44F5E7658F6B247A0C54A21057F7AE'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 a0 ae 44 f5 e7 65 8f 6b 24 7a 0c 54 a2 10 57 f7 ae

- No.: 2929
- Timestamp: 20:49:05:463_1
- RFN: 3751
- Chip: 2560
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2932
- Timestamp: 20:49:05:470_0
- RFN: 3751
- Chip: 28416
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_18:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000010101'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '44F5E7658F6B247A0C54A21057F7AE'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 a9 1e 44 f5 e7 65 8f 6b 24 7a 0c 54 a2 10 57 f7 ae

- No.: 2943
- Timestamp: 20:49:05:483_2
- RFN: 3753
- Chip: 4352
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2946
- Timestamp: 20:49:05:487_1
- RFN: 3753
- Chip: 17664
- Event: Timeout
- Source: tc_7_2_3_18:lt_TxAndRx LINE 5
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 2966
- Timestamp: 20:49:05:527_0
- RFN: 3757
- Chip: 14080
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000001100'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'EDE49A16FDB36D2485EA3107D59DC3'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 61 1e ed e4 9a 16 fd b3 6d 24 85 ea 31 07 d5 9d c3

- No.: 2975
- Timestamp: 20:49:05:542_1
- RFN: 3758
- Chip: 35328
- Event: Start Timer
- Source: tc_7_2_3_18:lt_TxAndRx LINE 9
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 2976
- Timestamp: 20:49:05:543_0
- RFN: 3758
- Chip: 36352
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2979
- Timestamp: 20:49:05:551_0
- RFN: 3759
- Chip: 32512
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_18:lt_TxAndRx LINE 3
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000010110'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . (AM_Data)data[16] = '3278595C235077F267A59097E8CEB432'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 b0 32 78 59 5c 23 50 77 f2 67 a5 90 97 e8 ce b4 32

- No.: 2990
- Timestamp: 20:49:05:567_1
- RFN: 3761
- Chip: 15104
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2993
- Timestamp: 20:49:05:574_0
- RFN: 3762
- Chip: 2048
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_18:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000010111'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '78595C235077F267A59097E8CEB432'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 b9 1e 78 59 5c 23 50 77 f2 67 a5 90 97 e8 ce b4 32

- No.: 3004
- Timestamp: 20:49:05:587_2
- RFN: 3763
- Chip: 15872
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3007
- Timestamp: 20:49:05:590_1
- RFN: 3763
- Chip: 28672
- Event: Timeout
- Source: tc_7_2_3_18:lt_TxAndRx LINE 5
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 3027
- Timestamp: 20:49:05:630_0
- RFN: 3767
- Chip: 25600
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000001101'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '60700D5488BEB9B96C24AF44DF498B'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 69 1e 60 70 0d 54 88 be b9 b9 6c 24 af 44 df 49 8b

- No.: 3036
- Timestamp: 20:49:05:643_0
- RFN: 3769
- Chip: 512
- Event: Start Timer
- Source: tc_7_2_3_18:lt_TxAndRx LINE 9
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 3037
- Timestamp: 20:49:05:643_1
- RFN: 3769
- Chip: 1280
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3042
- Timestamp: 20:49:05:657_1
- RFN: 3770
- Chip: 15616
- Event: Timeout
- Source: tc_7_2_3_18:lt_TxAndRx LINE 5
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 3062
- Timestamp: 20:49:05:701_0
- RFN: 3774
- Chip: 31744
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000001110'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'C135788C14A8BBEC64A5EF64DA1C56'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 71 1e c1 35 78 8c 14 a8 bb ec 64 a5 ef 64 da 1c 56

- No.: 3071
- Timestamp: 20:49:05:714_1
- RFN: 3776
- Chip: 6144
- Event: Start Timer
- Source: tc_7_2_3_18:lt_TxAndRx LINE 9
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 3072
- Timestamp: 20:49:05:714_2
- RFN: 3776
- Chip: 6912
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3075
- Timestamp: 20:49:05:723_0
- RFN: 3777
- Chip: 1024
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_18:lt_TxAndRx LINE 3
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000011000'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . (AM_Data)data[16] = 'EDE49A16FDB36D2485EA3107D59DC3ED'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 c0 ed e4 9a 16 fd b3 6d 24 85 ea 31 07 d5 9d c3 ed

- No.: 3086
- Timestamp: 20:49:05:737_1
- RFN: 3778
- Chip: 17152
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3089
- Timestamp: 20:49:05:743_0
- RFN: 3779
- Chip: 3840
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_18:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000011001'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = 'E49A16FDB36D2485EA3107D59DC3ED'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 c9 1e e4 9a 16 fd b3 6d 24 85 ea 31 07 d5 9d c3 ed

- No.: 3100
- Timestamp: 20:49:05:757_1
- RFN: 3780
- Chip: 17152
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3103
- Timestamp: 20:49:05:760_1
- RFN: 3780
- Chip: 30208
- Event: Timeout
- Source: tc_7_2_3_18:lt_TxAndRx LINE 5
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 3123
- Timestamp: 20:49:05:802_0
- RFN: 3785
- Chip: 0
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000001111'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '08FEB312D7B738D3E2CFB4C74A7458'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 79 1e 08 fe b3 12 d7 b7 38 d3 e2 cf b4 c7 4a 74 58

- No.: 3132
- Timestamp: 20:49:05:818_1
- RFN: 3786
- Chip: 22272
- Event: Start Timer
- Source: tc_7_2_3_18:lt_TxAndRx LINE 9
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 3133
- Timestamp: 20:49:05:818_2
- RFN: 3786
- Chip: 23296
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3136
- Timestamp: 20:49:05:826_0
- RFN: 3787
- Chip: 16896
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_18:lt_TxAndRx LINE 3
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000011010'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . (AM_Data)data[16] = '60700D5488BEB9B96C24AF44DF498B60'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 d0 60 70 0d 54 88 be b9 b9 6c 24 af 44 df 49 8b 60

- No.: 3147
- Timestamp: 20:49:05:841_1
- RFN: 3788
- Chip: 29952
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3150
- Timestamp: 20:49:05:848_0
- RFN: 3789
- Chip: 17408
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_18:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000011011'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '700D5488BEB9B96C24AF44DF498B60'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 d9 1e 70 0d 54 88 be b9 b9 6c 24 af 44 df 49 8b 60

- No.: 3161
- Timestamp: 20:49:05:863_2
- RFN: 3791
- Chip: 1024
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3164
- Timestamp: 20:49:05:874_0
- RFN: 3792
- Chip: 3840
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_18:lt_TxAndRx LINE 3
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000011100'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . (AM_Data)data[16] = 'C135788C14A8BBEC64A5EF64DA1C56C1'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 e0 c1 35 78 8c 14 a8 bb ec 64 a5 ef 64 da 1c 56 c1

- No.: 3175
- Timestamp: 20:49:05:887_2
- RFN: 3793
- Chip: 16640
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3178
- Timestamp: 20:49:05:894_0
- RFN: 3794
- Chip: 4096
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_18:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000011101'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '35788C14A8BBEC64A5EF64DA1C56C1'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 e9 1e 35 78 8c 14 a8 bb ec 64 a5 ef 64 da 1c 56 c1

- No.: 3189
- Timestamp: 20:49:05:908_1
- RFN: 3795
- Chip: 18432
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3192
- Timestamp: 20:49:05:911_1
- RFN: 3795
- Chip: 31744
- Event: Timeout
- Source: tc_7_2_3_18:lt_TxAndRx LINE 5
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 3212
- Timestamp: 20:49:05:952_0
- RFN: 3799
- Chip: 35840
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000010000'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'A3EF9B3C79F3CD348740DFE330780C'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 81 1e a3 ef 9b 3c 79 f3 cd 34 87 40 df e3 30 78 0c

- No.: 3221
- Timestamp: 20:49:05:966_0
- RFN: 3801
- Chip: 11520
- Event: Start Timer
- Source: tc_7_2_3_18:lt_TxAndRx LINE 9
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 3222
- Timestamp: 20:49:05:966_1
- RFN: 3801
- Chip: 12288
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3225
- Timestamp: 20:49:05:976_0
- RFN: 3802
- Chip: 14336
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_18:lt_TxAndRx LINE 3
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000011110'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . (AM_Data)data[16] = '08FEB312D7B738D3E2CFB4C74A745808'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 f0 08 fe b3 12 d7 b7 38 d3 e2 cf b4 c7 4a 74 58 08

- No.: 3236
- Timestamp: 20:49:05:990_2
- RFN: 3803
- Chip: 28672
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3239
- Timestamp: 20:49:05:997_0
- RFN: 3804
- Chip: 16384
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_18:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000011111'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = 'FEB312D7B738D3E2CFB4C74A745808'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 fd 1e fe b3 12 d7 b7 38 d3 e2 cf b4 c7 4a 74 58 08

- No.: 3244
- Timestamp: 20:49:06:010_0
- RFN: 3805
- Chip: 28416
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: tc_7_2_3_18:lt_CheckPollBit LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. STATUS_PDU
. . (DC_Field)dC_Field[1] = '0'B
. . (CtrlPDU_Type)type[3] = '000'B
. . SuperFields
. . . SUFI_WindowSize
. . . SUFI_List
. . . SUFI_RList
. . . SUFI_Bitmap
. . . SUFI_MRW
. . . SUFI_MRW_ACK
. . . SUFI_NoMore
. . . SUFI_Ack
. . . . (SUFI_Type)type[4] = '0010'B
. . . . (AM_SeqNum)lsn[12] = '000000100000'B
. . (HexStringType)superFieldsAndPadRx[-1] = -
. . (Padding)paddingTx[-1] = '0000000000000000000000000000000'H
- Constraint:
cas_StatusReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 02 02 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00

- No.: 3246
- Timestamp: 20:49:06:014_1
- RFN: 3806
- Chip: 4608
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: tc_7_2_3_18:lt_CheckPollBit LINE 5
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3254
- Timestamp: 20:49:06:024_0
- RFN: 3807
- Chip: 3584
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3257
- Timestamp: 20:49:06:027_1
- RFN: 3807
- Chip: 16896
- Event: Timeout
- Source: tc_7_2_3_18:lt_TxAndRx LINE 5
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 3277
- Timestamp: 20:49:06:066_0
- RFN: 3811
- Chip: 13312
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000010001'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '01FFCCCB4B8B9468A410A81157DD9C'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 89 1e 01 ff cc cb 4b 8b 94 68 a4 10 a8 11 57 dd 9c

- No.: 3286
- Timestamp: 20:49:06:079_1
- RFN: 3812
- Chip: 26368
- Event: Start Timer
- Source: tc_7_2_3_18:lt_TxAndRx LINE 9
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 3287
- Timestamp: 20:49:06:080_0
- RFN: 3812
- Chip: 27392
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3292
- Timestamp: 20:49:06:098_0
- RFN: 3814
- Chip: 20736
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_18:lt_TxAndRx LINE 3
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000100000'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . (AM_Data)data[16] = 'A3EF9B3C79F3CD348740DFE330780CA3'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 00 a3 ef 9b 3c 79 f3 cd 34 87 40 df e3 30 78 0c a3

- No.: 3303
- Timestamp: 20:49:06:114_0
- RFN: 3816
- Chip: 5376
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3306
- Timestamp: 20:49:06:120_0
- RFN: 3816
- Chip: 30976
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_18:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000100001'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = 'EF9B3C79F3CD348740DFE330780CA3'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 09 1e ef 9b 3c 79 f3 cd 34 87 40 df e3 30 78 0c a3

- No.: 3317
- Timestamp: 20:49:06:133_2
- RFN: 3818
- Chip: 4352
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3320
- Timestamp: 20:49:06:137_0
- RFN: 3818
- Chip: 17920
- Event: Timeout
- Source: tc_7_2_3_18:lt_TxAndRx LINE 5
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 3340
- Timestamp: 20:49:06:177_0
- RFN: 3822
- Chip: 15360
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000010010'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '9617027FA66F0E7E59A3C535D237AD'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 91 1e 96 17 02 7f a6 6f 0e 7e 59 a3 c5 35 d2 37 ad

- No.: 3349
- Timestamp: 20:49:06:190_1
- RFN: 3823
- Chip: 28416
- Event: Start Timer
- Source: tc_7_2_3_18:lt_TxAndRx LINE 9
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 3350
- Timestamp: 20:49:06:191_0
- RFN: 3823
- Chip: 29184
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3355
- Timestamp: 20:49:06:219_0
- RFN: 3826
- Chip: 23808
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_18:lt_TxAndRx LINE 3
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000100010'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . (AM_Data)data[16] = '01FFCCCB4B8B9468A410A81157DD9C01'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 10 01 ff cc cb 4b 8b 94 68 a4 10 a8 11 57 dd 9c 01

- No.: 3366
- Timestamp: 20:49:06:233_1
- RFN: 3828
- Chip: 0
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3369
- Timestamp: 20:49:06:238_0
- RFN: 3828
- Chip: 18688
- Event: Timeout
- Source: tc_7_2_3_18:lt_TxAndRx LINE 5
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 3389
- Timestamp: 20:49:06:277_0
- RFN: 3832
- Chip: 15872
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000010011'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '91C29FBCC61F032AD11D7C8CBE1302'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 99 1e 91 c2 9f bc c6 1f 03 2a d1 1d 7c 8c be 13 02

- No.: 3398
- Timestamp: 20:49:06:290_1
- RFN: 3833
- Chip: 27648
- Event: Start Timer
- Source: tc_7_2_3_18:lt_TxAndRx LINE 9
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 3399
- Timestamp: 20:49:06:290_2
- RFN: 3833
- Chip: 28672
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3402
- Timestamp: 20:49:06:297_0
- RFN: 3834
- Chip: 17664
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_18:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000100011'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = 'FFCCCB4B8B9468A410A81157DD9C01'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 19 1e ff cc cb 4b 8b 94 68 a4 10 a8 11 57 dd 9c 01

- No.: 3413
- Timestamp: 20:49:06:312_0
- RFN: 3835
- Chip: 34304
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3416
- Timestamp: 20:49:06:315_1
- RFN: 3836
- Chip: 8960
- Event: Timeout
- Source: tc_7_2_3_18:lt_TxAndRx LINE 5
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 3436
- Timestamp: 20:49:06:359_0
- RFN: 3840
- Chip: 26624
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000010100'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'D51DD637072A7BA6C5B5C760DAB6ED'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 a1 1e d5 1d d6 37 07 2a 7b a6 c5 b5 c7 60 da b6 ed

- No.: 3445
- Timestamp: 20:49:06:373_0
- RFN: 3842
- Chip: 0
- Event: Start Timer
- Source: tc_7_2_3_18:lt_TxAndRx LINE 9
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 3446
- Timestamp: 20:49:06:373_1
- RFN: 3842
- Chip: 1024
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3449
- Timestamp: 20:49:06:381_0
- RFN: 3842
- Chip: 33792
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_18:lt_TxAndRx LINE 3
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000100100'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . (AM_Data)data[16] = '9617027FA66F0E7E59A3C535D237AD96'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 20 96 17 02 7f a6 6f 0e 7e 59 a3 c5 35 d2 37 ad 96

- No.: 3460
- Timestamp: 20:49:06:395_1
- RFN: 3844
- Chip: 8960
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3463
- Timestamp: 20:49:06:401_0
- RFN: 3844
- Chip: 34816
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_18:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000100101'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '17027FA66F0E7E59A3C535D237AD96'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 29 1e 17 02 7f a6 6f 0e 7e 59 a3 c5 35 d2 37 ad 96

- No.: 3474
- Timestamp: 20:49:06:415_0
- RFN: 3846
- Chip: 8960
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3477
- Timestamp: 20:49:06:418_1
- RFN: 3846
- Chip: 22272
- Event: Timeout
- Source: tc_7_2_3_18:lt_TxAndRx LINE 5
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 3497
- Timestamp: 20:49:06:463_0
- RFN: 3851
- Chip: 0
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000010101'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'B1C7CA610FD4C8B41202FFB3387959'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 a9 1e b1 c7 ca 61 0f d4 c8 b4 12 02 ff b3 38 79 59

- No.: 3506
- Timestamp: 20:49:06:476_1
- RFN: 3852
- Chip: 12288
- Event: Start Timer
- Source: tc_7_2_3_18:lt_TxAndRx LINE 9
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 3507
- Timestamp: 20:49:06:477_0
- RFN: 3852
- Chip: 13312
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3510
- Timestamp: 20:49:06:485_0
- RFN: 3853
- Chip: 6912
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_18:lt_TxAndRx LINE 3
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000100110'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . (AM_Data)data[16] = '91C29FBCC61F032AD11D7C8CBE130291'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 30 91 c2 9f bc c6 1f 03 2a d1 1d 7c 8c be 13 02 91

- No.: 3521
- Timestamp: 20:49:06:499_1
- RFN: 3854
- Chip: 21760
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3524
- Timestamp: 20:49:06:505_0
- RFN: 3855
- Chip: 8704
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_18:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000100111'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = 'C29FBCC61F032AD11D7C8CBE130291'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 39 1e c2 9f bc c6 1f 03 2a d1 1d 7c 8c be 13 02 91

- No.: 3535
- Timestamp: 20:49:06:521_2
- RFN: 3856
- Chip: 31232
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3538
- Timestamp: 20:49:06:532_0
- RFN: 3857
- Chip: 34304
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_18:lt_TxAndRx LINE 3
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000101000'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . (AM_Data)data[16] = 'D51DD637072A7BA6C5B5C760DAB6EDD5'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 40 d5 1d d6 37 07 2a 7b a6 c5 b5 c7 60 da b6 ed d5

- No.: 3549
- Timestamp: 20:49:06:545_1
- RFN: 3859
- Chip: 8704
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3552
- Timestamp: 20:49:06:552_0
- RFN: 3859
- Chip: 34304
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_18:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000101001'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '1DD637072A7BA6C5B5C760DAB6EDD5'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 49 1e 1d d6 37 07 2a 7b a6 c5 b5 c7 60 da b6 ed d5

- No.: 3563
- Timestamp: 20:49:06:566_1
- RFN: 3861
- Chip: 11264
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3566
- Timestamp: 20:49:06:569_1
- RFN: 3861
- Chip: 24320
- Event: Timeout
- Source: tc_7_2_3_18:lt_TxAndRx LINE 5
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 3586
- Timestamp: 20:49:06:608_0
- RFN: 3865
- Chip: 21504
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000010110'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '768DBE39AC3B53886BF13287BF3986'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 b1 1e 76 8d be 39 ac 3b 53 88 6b f1 32 87 bf 39 86

- No.: 3595
- Timestamp: 20:49:06:624_0
- RFN: 3867
- Chip: 4352
- Event: Start Timer
- Source: tc_7_2_3_18:lt_TxAndRx LINE 9
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 3596
- Timestamp: 20:49:06:624_1
- RFN: 3867
- Chip: 5376
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3599
- Timestamp: 20:49:06:635_0
- RFN: 3868
- Chip: 7680
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_18:lt_TxAndRx LINE 3
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000101010'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . (AM_Data)data[16] = 'B1C7CA610FD4C8B41202FFB3387959B1'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 50 b1 c7 ca 61 0f d4 c8 b4 12 02 ff b3 38 79 59 b1

- No.: 3610
- Timestamp: 20:49:06:648_2
- RFN: 3869
- Chip: 21760
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3613
- Timestamp: 20:49:06:655_0
- RFN: 3870
- Chip: 9472
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_18:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000101011'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = 'C7CA610FD4C8B41202FFB3387959B1'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 59 1e c7 ca 61 0f d4 c8 b4 12 02 ff b3 38 79 59 b1

- No.: 3624
- Timestamp: 20:49:06:668_2
- RFN: 3871
- Chip: 21760
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3627
- Timestamp: 20:49:06:672_0
- RFN: 3871
- Chip: 34816
- Event: Timeout
- Source: tc_7_2_3_18:lt_TxAndRx LINE 5
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 3647
- Timestamp: 20:49:06:712_0
- RFN: 3875
- Chip: 35328
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000010111'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '95BDC635ADC49F43207AA6EF1B292E'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 b9 1e 95 bd c6 35 ad c4 9f 43 20 7a a6 ef 1b 29 2e

- No.: 3656
- Timestamp: 20:49:06:725_1
- RFN: 3877
- Chip: 10240
- Event: Start Timer
- Source: tc_7_2_3_18:lt_TxAndRx LINE 9
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 3657
- Timestamp: 20:49:06:725_2
- RFN: 3877
- Chip: 11008
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3662
- Timestamp: 20:49:06:742_0
- RFN: 3878
- Chip: 36608
- Event: Timeout
- Source: tc_7_2_3_18:lt_TxAndRx LINE 5
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 3682
- Timestamp: 20:49:06:787_0
- RFN: 3883
- Chip: 16128
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000011000'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '84EA1BA93BD39D3C8615A891428AEB'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 c1 1e 84 ea 1b a9 3b d3 9d 3c 86 15 a8 91 42 8a eb

- No.: 3691
- Timestamp: 20:49:06:801_0
- RFN: 3884
- Chip: 28672
- Event: Start Timer
- Source: tc_7_2_3_18:lt_TxAndRx LINE 9
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 3692
- Timestamp: 20:49:06:801_1
- RFN: 3884
- Chip: 29440
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3695
- Timestamp: 20:49:06:809_0
- RFN: 3885
- Chip: 23808
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_18:lt_TxAndRx LINE 3
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000101100'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . (AM_Data)data[16] = '768DBE39AC3B53886BF13287BF398676'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 60 76 8d be 39 ac 3b 53 88 6b f1 32 87 bf 39 86 76

- No.: 3706
- Timestamp: 20:49:06:823_1
- RFN: 3886
- Chip: 38144
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3709
- Timestamp: 20:49:06:830_0
- RFN: 3887
- Chip: 25600
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_18:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000101101'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '8DBE39AC3B53886BF13287BF398676'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 69 1e 8d be 39 ac 3b 53 88 6b f1 32 87 bf 39 86 76

- No.: 3720
- Timestamp: 20:49:06:843_1
- RFN: 3888
- Chip: 38144
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3723
- Timestamp: 20:49:06:846_1
- RFN: 3889
- Chip: 13056
- Event: Timeout
- Source: tc_7_2_3_18:lt_TxAndRx LINE 5
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 3743
- Timestamp: 20:49:06:888_0
- RFN: 3893
- Chip: 20992
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000011001'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'B1382C04AA110280400AABBB939797'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 c9 1e b1 38 2c 04 aa 11 02 80 40 0a ab bb 93 97 97

- No.: 3752
- Timestamp: 20:49:06:904_0
- RFN: 3895
- Chip: 3584
- Event: Start Timer
- Source: tc_7_2_3_18:lt_TxAndRx LINE 9
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 3753
- Timestamp: 20:49:06:904_1
- RFN: 3895
- Chip: 4608
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3756
- Timestamp: 20:49:06:912_0
- RFN: 3895
- Chip: 36608
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_18:lt_TxAndRx LINE 3
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000101110'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . (AM_Data)data[16] = '95BDC635ADC49F43207AA6EF1B292E95'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 70 95 bd c6 35 ad c4 9f 43 20 7a a6 ef 1b 29 2e 95

- No.: 3767
- Timestamp: 20:49:06:926_0
- RFN: 3897
- Chip: 11776
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3770
- Timestamp: 20:49:06:935_0
- RFN: 3898
- Chip: 8960
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_18:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000101111'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = 'BDC635ADC49F43207AA6EF1B292E95'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 79 1e bd c6 35 ad c4 9f 43 20 7a a6 ef 1b 29 2e 95

- No.: 3781
- Timestamp: 20:49:06:951_1
- RFN: 3899
- Chip: 31232
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3784
- Timestamp: 20:49:06:959_0
- RFN: 3900
- Chip: 26112
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_18:lt_TxAndRx LINE 3
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000110000'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . (AM_Data)data[16] = '84EA1BA93BD39D3C8615A891428AEB84'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 80 84 ea 1b a9 3b d3 9d 3c 86 15 a8 91 42 8a eb 84

- No.: 3795
- Timestamp: 20:49:06:973_0
- RFN: 3902
- Chip: 0
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3798
- Timestamp: 20:49:06:979_0
- RFN: 3902
- Chip: 25856
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_18:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000110001'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = 'EA1BA93BD39D3C8615A891428AEB84'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 89 1e ea 1b a9 3b d3 9d 3c 86 15 a8 91 42 8a eb 84

- No.: 3809
- Timestamp: 20:49:06:993_1
- RFN: 3904
- Chip: 2048
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3812
- Timestamp: 20:49:06:997_0
- RFN: 3904
- Chip: 15360
- Event: Timeout
- Source: tc_7_2_3_18:lt_TxAndRx LINE 5
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 3832
- Timestamp: 20:49:07:038_0
- RFN: 3908
- Chip: 22272
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000011010'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '3D863F067F0CD4B74720D01D562250'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 d1 1e 3d 86 3f 06 7f 0c d4 b7 47 20 d0 1d 56 22 50

- No.: 3841
- Timestamp: 20:49:07:054_1
- RFN: 3910
- Chip: 6656
- Event: Start Timer
- Source: tc_7_2_3_18:lt_TxAndRx LINE 9
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 3842
- Timestamp: 20:49:07:054_2
- RFN: 3910
- Chip: 7424
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3845
- Timestamp: 20:49:07:063_0
- RFN: 3911
- Chip: 1280
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_18:lt_TxAndRx LINE 3
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000110010'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . (AM_Data)data[16] = 'B1382C04AA110280400AABBB939797B1'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 90 b1 38 2c 04 aa 11 02 80 40 0a ab bb 93 97 97 b1

- No.: 3856
- Timestamp: 20:49:07:076_0
- RFN: 3912
- Chip: 13312
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3859
- Timestamp: 20:49:07:083_0
- RFN: 3913
- Chip: 1536
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_18:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000110011'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '382C04AA110280400AABBB939797B1'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 99 1e 38 2c 04 aa 11 02 80 40 0a ab bb 93 97 97 b1

- No.: 3870
- Timestamp: 20:49:07:097_1
- RFN: 3914
- Chip: 13824
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3873
- Timestamp: 20:49:07:100_1
- RFN: 3914
- Chip: 27136
- Event: Timeout
- Source: tc_7_2_3_18:lt_TxAndRx LINE 5
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 3893
- Timestamp: 20:49:07:140_0
- RFN: 3918
- Chip: 25344
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000011011'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '5D5C89EBCECB1ED648F418A94420AF'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 d9 1e 5d 5c 89 eb ce cb 1e d6 48 f4 18 a9 44 20 af

- No.: 3902
- Timestamp: 20:49:07:153_1
- RFN: 3920
- Chip: 0
- Event: Start Timer
- Source: tc_7_2_3_18:lt_TxAndRx LINE 9
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 3903
- Timestamp: 20:49:07:153_2
- RFN: 3920
- Chip: 768
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3908
- Timestamp: 20:49:07:174_1
- RFN: 3922
- Chip: 3584
- Event: Timeout
- Source: tc_7_2_3_18:lt_TxAndRx LINE 5
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 3928
- Timestamp: 20:49:07:218_0
- RFN: 3926
- Chip: 21504
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000011100'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = 'EE64F0B2B846A0EFE4CF4B212FD19D'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 e1 1e ee 64 f0 b2 b8 46 a0 ef e4 cf 4b 21 2f d1 9d

- No.: 3937
- Timestamp: 20:49:07:232_0
- RFN: 3927
- Chip: 34048
- Event: Start Timer
- Source: tc_7_2_3_18:lt_TxAndRx LINE 9
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 3938
- Timestamp: 20:49:07:232_1
- RFN: 3927
- Chip: 35072
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3941
- Timestamp: 20:49:07:240_0
- RFN: 3928
- Chip: 28672
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_18:lt_TxAndRx LINE 3
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000110100'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . (AM_Data)data[16] = '3D863F067F0CD4B74720D01D5622503D'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 a0 3d 86 3f 06 7f 0c d4 b7 47 20 d0 1d 56 22 50 3d

- No.: 3952
- Timestamp: 20:49:07:254_0
- RFN: 3930
- Chip: 3584
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3955
- Timestamp: 20:49:07:260_0
- RFN: 3930
- Chip: 28416
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_18:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000110101'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '863F067F0CD4B74720D01D5622503D'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 a9 1e 86 3f 06 7f 0c d4 b7 47 20 d0 1d 56 22 50 3d

- No.: 3966
- Timestamp: 20:49:07:273_2
- RFN: 3932
- Chip: 3072
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 3969
- Timestamp: 20:49:07:277_0
- RFN: 3932
- Chip: 16128
- Event: Timeout
- Source: tc_7_2_3_18:lt_TxAndRx LINE 5
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 3989
- Timestamp: 20:49:07:321_0
- RFN: 3936
- Chip: 33536
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000011101'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '69DBC9342DFB66DA490BD4620FAB3B'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 e9 1e 69 db c9 34 2d fb 66 da 49 0b d4 62 0f ab 3b

- No.: 3998
- Timestamp: 20:49:07:335_0
- RFN: 3938
- Chip: 8448
- Event: Start Timer
- Source: tc_7_2_3_18:lt_TxAndRx LINE 9
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 3999
- Timestamp: 20:49:07:335_1
- RFN: 3938
- Chip: 9216
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4002
- Timestamp: 20:49:07:343_0
- RFN: 3939
- Chip: 2560
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_18:lt_TxAndRx LINE 3
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000110110'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . (AM_Data)data[16] = '5D5C89EBCECB1ED648F418A94420AF5D'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 b0 5d 5c 89 eb ce cb 1e d6 48 f4 18 a9 44 20 af 5d

- No.: 4013
- Timestamp: 20:49:07:357_0
- RFN: 3940
- Chip: 16384
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4016
- Timestamp: 20:49:07:363_0
- RFN: 3941
- Chip: 3840
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_18:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000110111'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '5C89EBCECB1ED648F418A94420AF5D'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 b9 1e 5c 89 eb ce cb 1e d6 48 f4 18 a9 44 20 af 5d

- No.: 4027
- Timestamp: 20:49:07:379_2
- RFN: 3942
- Chip: 26112
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4030
- Timestamp: 20:49:07:387_0
- RFN: 3943
- Chip: 19968
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_18:lt_TxAndRx LINE 3
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000111000'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . (AM_Data)data[16] = 'EE64F0B2B846A0EFE4CF4B212FD19DEE'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 c0 ee 64 f0 b2 b8 46 a0 ef e4 cf 4b 21 2f d1 9d ee

- No.: 4041
- Timestamp: 20:49:07:404_1
- RFN: 3945
- Chip: 3328
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4044
- Timestamp: 20:49:07:411_0
- RFN: 3945
- Chip: 29440
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_18:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000111001'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '64F0B2B846A0EFE4CF4B212FD19DEE'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 c9 1e 64 f0 b2 b8 46 a0 ef e4 cf 4b 21 2f d1 9d ee

- No.: 4055
- Timestamp: 20:49:07:425_0
- RFN: 3947
- Chip: 5888
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4058
- Timestamp: 20:49:07:428_1
- RFN: 3947
- Chip: 18688
- Event: Timeout
- Source: tc_7_2_3_18:lt_TxAndRx LINE 5
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 4078
- Timestamp: 20:49:07:467_0
- RFN: 3951
- Chip: 15872
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000011110'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '86C0E01AA9117D7372D8495E89BE93'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 f1 1e 86 c0 e0 1a a9 11 7d 73 72 d8 49 5e 89 be 93

- No.: 4087
- Timestamp: 20:49:07:483_0
- RFN: 3952
- Chip: 38144
- Event: Start Timer
- Source: tc_7_2_3_18:lt_TxAndRx LINE 9
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 4088
- Timestamp: 20:49:07:483_1
- RFN: 3953
- Chip: 768
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4091
- Timestamp: 20:49:07:494_0
- RFN: 3954
- Chip: 3584
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_18:lt_TxAndRx LINE 3
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000111010'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . (AM_Data)data[16] = '69DBC9342DFB66DA490BD4620FAB3B69'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 d0 69 db c9 34 2d fb 66 da 49 0b d4 62 0f ab 3b 69

- No.: 4102
- Timestamp: 20:49:07:507_2
- RFN: 3955
- Chip: 17152
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4105
- Timestamp: 20:49:07:514_0
- RFN: 3956
- Chip: 5376
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_18:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000111011'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = 'DBC9342DFB66DA490BD4620FAB3B69'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 d9 1e db c9 34 2d fb 66 da 49 0b d4 62 0f ab 3b 69

- No.: 4116
- Timestamp: 20:49:07:528_0
- RFN: 3957
- Chip: 18176
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4119
- Timestamp: 20:49:07:531_1
- RFN: 3957
- Chip: 31232
- Event: Timeout
- Source: tc_7_2_3_18:lt_TxAndRx LINE 5
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 4139
- Timestamp: 20:49:07:570_0
- RFN: 3961
- Chip: 28160
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: ts_TxAMD_PRBS LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000011111'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[-1] = '17826AF118295177D8C94BDEC9B438'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[-1] = -
- Constraint:
cas_DataReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 80 f9 1e 17 82 6a f1 18 29 51 77 d8 c9 4b de c9 b4 38

- No.: 4148
- Timestamp: 20:49:07:583_1
- RFN: 3963
- Chip: 2304
- Event: Start Timer
- Source: tc_7_2_3_18:lt_TxAndRx LINE 9
- Message Structure:
no details available
- Constraint:
t_TTI (20 Ms)
- BinaryMessage:

- No.: 4149
- Timestamp: 20:49:07:583_2
- RFN: 3963
- Chip: 3328
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4154
- Timestamp: 20:49:07:596_0
- RFN: 3964
- Chip: 12032
- Event: Timeout
- Source: tc_7_2_3_18:lt_TxAndRx LINE 5
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 4156
- Timestamp: 20:49:07:599_0
- RFN: 3964
- Chip: 23296
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4161
- Timestamp: 20:49:07:619_0
- RFN: 3966
- Chip: 23552
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_18:lt_TxAndRx LINE 3
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000111100'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . (AM_Data)data[16] = '86C0E01AA9117D7372D8495E89BE9386'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 e0 86 c0 e0 1a a9 11 7d 73 72 d8 49 5e 89 be 93 86

- No.: 4172
- Timestamp: 20:49:07:635_0
- RFN: 3968
- Chip: 7936
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4175
- Timestamp: 20:49:07:641_0
- RFN: 3968
- Chip: 34304
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_18:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000111101'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = 'C0E01AA9117D7372D8495E89BE9386'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 e9 1e c0 e0 1a a9 11 7d 73 72 d8 49 5e 89 be 93 86

- No.: 4186
- Timestamp: 20:49:07:654_2
- RFN: 3970
- Chip: 7680
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4191
- Timestamp: 20:49:07:719_0
- RFN: 3976
- Chip: 23808
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_18:lt_TxAndRx LINE 3
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000111110'B
. . (PollingBit)pollingBit[1] = '0'B
. . (HeaderExt)headerExt[2] = '00'B
. . LenInds
. . (AM_Data)data[16] = '17826AF118295177D8C94BDEC9B43817'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 f0 17 82 6a f1 18 29 51 77 d8 c9 4b de c9 b4 38 17

- No.: 4202
- Timestamp: 20:49:07:733_1
- RFN: 3977
- Chip: 37888
- Event: Repeat
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 6
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4207
- Timestamp: 20:49:07:744_0
- RFN: 3979
- Chip: 4608
- Event: Receive
- PCO: TM
- Message: RLC_TR_TestDataInd
- Source: tc_7_2_3_18:lt_TxAndRx LINE 1
- Message Structure:
RLC_TR_TestDataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. AMD_PDU
. . (DC_Field)dcField[1] = '1'B
. . (AM_SeqNum)seqNum[12] = '000000111111'B
. . (PollingBit)pollingBit[1] = '1'B
. . (HeaderExt)headerExt[2] = '01'B
. . LenInds
. . . LenInd7AndE_Bit
. . . . (LenInd7)lenInd[7] = '0001111'B
. . . . (ExtBit)extBit[1] = '0'B
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd7AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . . LenInd15AndE_Bit
. . (AM_Data)data[15] = '826AF118295177D8C94BDEC9B43817'O
. . PiggyBackedSTATUS_PDU
. . (Padding)padding[0] = -
- Constraint:
car_DataInd
- BinaryMessage:
ff ff ff ff ff ff ff f4 81 fd 1e 82 6a f1 18 29 51 77 d8 c9 4b de c9 b4 38 17

- No.: 4212
- Timestamp: 20:49:07:757_0
- RFN: 3980
- Chip: 13568
- Event: Send
- PCO: TM
- Message: RLC_TR_TestDataReq
- Source: tc_7_2_3_18:lt_CheckPollBit LINE 4
- Message Structure:
RLC_TR_TestDataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = -12
. STATUS_PDU
. . (DC_Field)dC_Field[1] = '0'B
. . (CtrlPDU_Type)type[3] = '000'B
. . SuperFields
. . . SUFI_WindowSize
. . . SUFI_List
. . . SUFI_RList
. . . SUFI_Bitmap
. . . SUFI_MRW
. . . SUFI_MRW_ACK
. . . SUFI_NoMore
. . . SUFI_Ack
. . . . (SUFI_Type)type[4] = '0010'B
. . . . (AM_SeqNum)lsn[12] = '000001000000'B
. . (HexStringType)superFieldsAndPadRx[-1] = -
. . (Padding)paddingTx[-1] = '0000000000000000000000000000000'H
- Constraint:
cas_StatusReq
- BinaryMessage:
ff ff ff ff ff ff ff f4 02 04 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00

- No.: 4214
- Timestamp: 20:49:07:760_1
- RFN: 3980
- Chip: 28160
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: tc_7_2_3_18:lt_CheckPollBit LINE 5
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4224
- Timestamp: 20:49:07:776_0
- RFN: 3982
- Chip: 11264
- Event: Cancel Timer
- Source: tc_7_2_3_18:lt_PollEveryPollSDU_Test LINE 8
- Message Structure:
no details available
- Constraint:
t_TTI
- BinaryMessage:

- No.: 4228
- Timestamp: 20:49:07:785_0
- RFN: 3983
- Chip: 5888
- Event: Send
- PCO: Dc
- Message: RRC_DataReq
- Source: ts_TC_OpenUE_TestLoop LINE 6
- Message Structure:
RRC_DataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[-1] = -
. (SapId)sapId[1] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. OPENUETESTLOOP
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)tCProtocolDiscriminator[4] = '1111'B
. . (MsgType)msgType[8] = '01000010'B
- Constraint:
ca_PS_DataReq
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 0f 42

- No.: 4229
- Timestamp: 20:49:07:785_1
- RFN: 3983
- Chip: 9216
- Event: Start Timer
- Source: ts_TC_OpenUE_TestLoop LINE 6
- Message Structure:
no details available
- Constraint:
t_Dly (5000 Ms)
- BinaryMessage:

- No.: 4233
- Timestamp: 20:49:08:057_0
- RFN: 4010
- Chip: 13568
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_TC_OpenUE_TestLoop LINE 7
- Message Structure:
RRC_DataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. (START_Value)start[0] = -
. OPENUETESTLOOPCOMPLETE
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)tCProtocolDiscriminator[4] = '1111'B
. . (MsgType)msgType[8] = '01000011'B
- Constraint:
car_PS_UplinkDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 0f 43

- No.: 4234
- Timestamp: 20:49:08:058_0
- RFN: 4010
- Chip: 16896
- Event: Cancel Timer
- Source: ts_TC_OpenUE_TestLoop LINE 7
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 4235
- Timestamp: 20:49:08:058_1
- RFN: 4010
- Chip: 17920
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_TC_OpenUE_TestLoop LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4247
- Timestamp: 20:49:08:066_0
- RFN: 4011
- Chip: 11520
- Event: Send
- PCO: Dc
- Message: RRC_DataReq
- Source: ts_TC_DeactivateRB_TestMode LINE 6
- Message Structure:
RRC_DataReq
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[-1] = -
. (SapId)sapId[1] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. DEACTIVATERBTESTMODE
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)tCProtocolDiscriminator[4] = '1111'B
. . (MsgType)msgType[8] = '01000110'B
- Constraint:
ca_PS_DataReq
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 0f 46

- No.: 4248
- Timestamp: 20:49:08:067_0
- RFN: 4011
- Chip: 14848
- Event: Start Timer
- Source: ts_TC_DeactivateRB_TestMode LINE 6
- Message Structure:
no details available
- Constraint:
t_Dly (5000 Ms)
- BinaryMessage:

- No.: 4252
- Timestamp: 20:49:08:374_0
- RFN: 4042
- Chip: 4352
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_TC_DeactivateRB_TestMode LINE 7
- Message Structure:
RRC_DataInd
. (IntegerType)cellId = -1
. (SS_RB_Identity)rB_Id = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain = 1
. (START_Value)start[0] = -
. DEACTIVATERBTESTMODECOMPLETE
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)tCProtocolDiscriminator[4] = '1111'B
. . (MsgType)msgType[8] = '01000111'B
- Constraint:
car_PS_UplinkDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 01 0f 47

- No.: 4253
- Timestamp: 20:49:08:375_0
- RFN: 4042
- Chip: 7680
- Event: Cancel Timer
- Source: ts_TC_DeactivateRB_TestMode LINE 7
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 4254
- Timestamp: 20:49:08:375_1
- RFN: 4042
- Chip: 8448
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_TC_DeactivateRB_TestMode LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4266
- Timestamp: 20:49:08:384_0
- RFN: 4043
- Chip: 2560
- Event: Send
- PCO: UM
- Message: RLC_UM_DATA_REQ
- Source: po_ConnectionAndSS_Rel:lt_Send_RRC_ConnectionRelease LINE 8
- Message Structure:
RLC_UM_DATA_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. uM_message
. . DL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00000000000000000000000000000000"
. . . . (IntegerType)rrc_MessageSequenceNumber = 0
. . . DL_DCCH_MessageType
. . . . RRCConnectionRelease
. . . . . r3
. . . . . . RRCConnectionRelease_r3_IEs
. . . . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . . . (IntegerType)n_308 = 1
. . . . . . . (ReleaseCause)releaseCause = 0
. . . . . . . Rplmn_Information
. . . . . . laterNonCriticalExtensions
. (BooleanType)specialLI = FALSE
- Constraint:
cas_RRC_ConnRelDCCH
- BinaryMessage:
30 10 02 01 ff 02 01 01 80 00 00 00 03 c8 00 01 01 00

- No.: 4270
- Timestamp: 20:49:08:615_0
- RFN: 4066
- Chip: 9216
- Event: Receive
- PCO: UM
- Message: RLC_UM_DATA_IND
- Source: po_ConnectionAndSS_Rel:lt_Send_RRC_ConnectionRelease LINE 9
- Message Structure:
RLC_UM_DATA_IND
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. IntegrityResult
. uM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "10110011101011111111101100111000"
. . . . (IntegerType)rrc_MessageSequenceNumber = 1
. . . UL_DCCH_MessageType
. . . . RRCConnectionReleaseComplete
. . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . FailureCauseWithProtErr
. . . . . laterNonCriticalExtensions
. . . . . . (BitStringType)rrcConnectionReleaseComplete_r3_add_ext = 0
. . . . . . nonCriticalExtensions
- Constraint:
car_RRC_ConnRelCmplUM
- BinaryMessage:
30 0c 02 01 ff 02 01 01 d9 d7 fd 9c 0c 40

- No.: 4271
- Timestamp: 20:49:08:616_0
- RFN: 4066
- Chip: 12800
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: po_ConnectionAndSS_Rel:lt_Send_RRC_ConnectionRelease LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4274
- Timestamp: 20:49:08:617_0
- RFN: 4066
- Chip: 17920
- Event: Start Timer
- Source: po_ConnectionAndSS_Rel:lt_RptRcvConnRel LINE 1
- Message Structure:
no details available
- Constraint:
t_Dly (5000 Ms)
- BinaryMessage:

- No.: 4278
- Timestamp: 20:49:08:775_0
- RFN: 4082
- Chip: 7936
- Event: Receive
- PCO: UM
- Message: RLC_UM_DATA_IND
- Source: po_ConnectionAndSS_Rel:lt_RptRcvConnRel LINE 4
- Message Structure:
RLC_UM_DATA_IND
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. IntegrityResult
. uM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00111001011111110001011000001001"
. . . . (IntegerType)rrc_MessageSequenceNumber = 2
. . . UL_DCCH_MessageType
. . . . RRCConnectionReleaseComplete
. . . . . (IntegerType)rrc_TransactionIdentifier = 0
. . . . . FailureCauseWithProtErr
. . . . . laterNonCriticalExtensions
. . . . . . (BitStringType)rrcConnectionReleaseComplete_r3_add_ext = 0
. . . . . . nonCriticalExtensions
- Constraint:
car_RRC_ConnRelCmplUM
- BinaryMessage:
30 0c 02 01 ff 02 01 01 9c bf 8b 04 94 40

- No.: 4279
- Timestamp: 20:49:08:776_0
- RFN: 4082
- Chip: 11776
- Event: Cancel Timer
- Source: po_ConnectionAndSS_Rel:lt_RptRcvConnRel LINE 4
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 4280
- Timestamp: 20:49:08:776_1
- RFN: 4082
- Chip: 12800
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: po_ConnectionAndSS_Rel:lt_RptRcvConnRel LINE 4
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4296
- Timestamp: 20:49:08:783_0
- RFN: 4082
- Chip: 37888
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 01 0a 01 00 05 00

- No.: 4300
- Timestamp: 20:49:08:792_0
- RFN: 4083
- Chip: 36096
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 4303
- Timestamp: 20:49:08:795_0
- RFN: 4084
- Chip: 9472
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 02 0a 01 00 05 00

- No.: 4307
- Timestamp: 20:49:08:804_0
- RFN: 4085
- Chip: 4864
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 4310
- Timestamp: 20:49:08:807_0
- RFN: 4085
- Chip: 16896
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 03 0a 01 00 05 00

- No.: 4314
- Timestamp: 20:49:08:814_0
- RFN: 4086
- Chip: 6656
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 3
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 4317
- Timestamp: 20:49:08:817_0
- RFN: 4086
- Chip: 17920
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 04 0a 01 00 05 00

- No.: 4321
- Timestamp: 20:49:08:824_0
- RFN: 4087
- Chip: 6656
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = 4
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 4327
- Timestamp: 20:49:08:828_0
- RFN: 4087
- Chip: 21248
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = -12
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 f4 0a 01 00 05 00

- No.: 4331
- Timestamp: 20:49:08:834_0
- RFN: 4088
- Chip: 4096
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)rB_Identity = -12
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 f4

- No.: 4335
- Timestamp: 20:49:08:843_0
- RFN: 4088
- Chip: 38144
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_CMAC_Rel LINE 1
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
. (RatType)ratType = 0
. configMessage
- Constraint:
cas_MAC_Rel
- BinaryMessage:
30 0b 02 01 ff 02 01 1a 0a 01 00 05 00

- No.: 4339
- Timestamp: 20:49:08:850_0
- RFN: 4089
- Chip: 29184
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_CMAC_Rel LINE 2
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 1a

- No.: 4342
- Timestamp: 20:49:08:857_0
- RFN: 4090
- Chip: 15360
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_CMAC_Rel LINE 1
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
. (RatType)ratType = 0
. configMessage
- Constraint:
cas_MAC_Rel
- BinaryMessage:
30 0b 02 01 ff 02 01 14 0a 01 00 05 00

- No.: 4346
- Timestamp: 20:49:08:863_0
- RFN: 4091
- Chip: 512
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_CMAC_Rel LINE 2
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId = -1
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 14

- No.: 4349
- Timestamp: 20:49:08:865_0
- RFN: 4091
- Chip: 11264
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Release_REQ
- Source: ts_CPHY_TrChRel LINE 1
- Message Structure:
CPHY_TrCH_Release_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
ca_PHY_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 1a

- No.: 4353
- Timestamp: 20:49:08:872_0
- RFN: 4091
- Chip: 35584
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Release_CNF
- Source: ts_CPHY_TrChRel LINE 2
- Message Structure:
CPHY_TrCH_Release_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
ca_PHY_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 1a

- No.: 4356
- Timestamp: 20:49:08:875_0
- RFN: 4092
- Chip: 7936
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Release_REQ
- Source: ts_CPHY_TrChRel LINE 1
- Message Structure:
CPHY_TrCH_Release_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_PHY_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 4361
- Timestamp: 20:49:08:880_0
- RFN: 4092
- Chip: 30720
- Event: Receive
- PCO: CPHY
- Message: CPHY_Out_of_Sync_IND
- Source: SS_Def LINE 5
- Message Structure:
CPHY_Out_of_Sync_IND
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_OutOfSyncInd
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 4362
- Timestamp: 20:49:08:881_0
- RFN: 4092
- Chip: 33792
- Event: Default
- Source: SS_Def LINE 0
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4363
- Timestamp: 20:49:08:882_0
- RFN: 4092
- Chip: 34816
- Event: Default
- Source: ts_CPHY_TrChRel LINE 2
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 4368
- Timestamp: 20:49:08:902_0
- RFN: 4094
- Chip: 36864
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Release_CNF
- Source: ts_CPHY_TrChRel LINE 2
- Message Structure:
CPHY_TrCH_Release_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_PHY_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 4371
- Timestamp: 20:49:08:905_0
- RFN: 4095
- Chip: 8960
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 1a

- No.: 4375
- Timestamp: 20:49:08:912_0
- RFN: 4095
- Chip: 38144
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 26
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 1a

- No.: 4378
- Timestamp: 20:49:08:915_0
- RFN: 4096
- Chip: 10752
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 4382
- Timestamp: 20:49:08:941_0
- RFN: 4098
- Chip: 34304
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 20
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 14

- No.: 4387
- Timestamp: 20:49:08:945_0
- RFN: 4099
- Chip: 8960
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 00 02 01 00 0a 01 00 05 00

- No.: 4391
- Timestamp: 20:49:08:951_0
- RFN: 4099
- Chip: 31744
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = 0
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 00

- No.: 4394
- Timestamp: 20:49:08:955_0
- RFN: 4100
- Chip: 9728
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_CMAC_Rel LINE 1
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 8
. (RatType)ratType = 0
. configMessage
- Constraint:
cas_MAC_Rel
- BinaryMessage:
30 0b 02 01 00 02 01 08 0a 01 00 05 00

- No.: 4398
- Timestamp: 20:49:08:961_0
- RFN: 4100
- Chip: 32000
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_CMAC_Rel LINE 2
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 8
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 08

- No.: 4401
- Timestamp: 20:49:08:963_0
- RFN: 4101
- Chip: 4608
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Release_REQ
- Source: ts_CPHY_TrChRel LINE 1
- Message Structure:
CPHY_TrCH_Release_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 8
- Constraint:
ca_PHY_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 08

- No.: 4405
- Timestamp: 20:49:08:992_0
- RFN: 4103
- Chip: 33280
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Release_CNF
- Source: ts_CPHY_TrChRel LINE 2
- Message Structure:
CPHY_TrCH_Release_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 8
- Constraint:
ca_PHY_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 08

- No.: 4408
- Timestamp: 20:49:08:995_0
- RFN: 4104
- Chip: 5888
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 7
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 07

- No.: 4412
- Timestamp: 20:49:09:001_0
- RFN: 4104
- Chip: 28928
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 7
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 07

- No.: 4415
- Timestamp: 20:49:09:003_0
- RFN: 4105
- Chip: 768
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 8
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 08

- No.: 4419
- Timestamp: 20:49:09:032_0
- RFN: 4107
- Chip: 33024
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 8
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 08

- No.: 4422
- Timestamp: 20:49:09:035_0
- RFN: 4108
- Chip: 6144
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -2
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 00 02 01 fe 0a 01 00 05 00

- No.: 4426
- Timestamp: 20:49:09:040_0
- RFN: 4108
- Chip: 26368
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 fe

- No.: 4429
- Timestamp: 20:49:09:044_0
- RFN: 4109
- Chip: 3072
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_CMAC_Rel LINE 1
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 5
. (RatType)ratType = 0
. configMessage
- Constraint:
cas_MAC_Rel
- BinaryMessage:
30 0b 02 01 00 02 01 05 0a 01 00 05 00

- No.: 4433
- Timestamp: 20:49:09:051_0
- RFN: 4109
- Chip: 29184
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_CMAC_Rel LINE 2
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 5
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 05

- No.: 4436
- Timestamp: 20:49:09:053_0
- RFN: 4110
- Chip: 256
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Release_REQ
- Source: ts_CPHY_TrChRel LINE 1
- Message Structure:
CPHY_TrCH_Release_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 5
- Constraint:
ca_PHY_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 05

- No.: 4440
- Timestamp: 20:49:09:060_0
- RFN: 4110
- Chip: 28160
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Release_CNF
- Source: ts_CPHY_TrChRel LINE 2
- Message Structure:
CPHY_TrCH_Release_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 5
- Constraint:
ca_PHY_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 05

- No.: 4443
- Timestamp: 20:49:09:063_0
- RFN: 4111
- Chip: 1792
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 6
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 06

- No.: 4447
- Timestamp: 20:49:09:070_0
- RFN: 4111
- Chip: 26880
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 6
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 06

- No.: 4450
- Timestamp: 20:49:09:072_0
- RFN: 4111
- Chip: 36864
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 5
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 05

- No.: 4454
- Timestamp: 20:49:09:080_0
- RFN: 4112
- Chip: 28672
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 5
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 05

- No.: 4459
- Timestamp: 20:49:09:084_0
- RFN: 4113
- Chip: 3072
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
. (RatType)ratType = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 00 02 01 ff 0a 01 00 05 00

- No.: 4463
- Timestamp: 20:49:09:089_0
- RFN: 4113
- Chip: 22528
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)rB_Identity = -1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 4466
- Timestamp: 20:49:09:092_0
- RFN: 4113
- Chip: 35072
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_CMAC_Rel LINE 1
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 4
. (RatType)ratType = 0
. configMessage
- Constraint:
cas_MAC_Rel
- BinaryMessage:
30 0b 02 01 00 02 01 04 0a 01 00 05 00

- No.: 4470
- Timestamp: 20:49:09:098_0
- RFN: 4114
- Chip: 20224
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_CMAC_Rel LINE 2
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 4
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 04

- No.: 4473
- Timestamp: 20:49:09:101_0
- RFN: 4114
- Chip: 30464
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Release_REQ
- Source: ts_CPHY_TrChRel LINE 1
- Message Structure:
CPHY_TrCH_Release_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 4
- Constraint:
ca_PHY_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 04

- No.: 4477
- Timestamp: 20:49:09:107_0
- RFN: 4115
- Chip: 15872
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Release_CNF
- Source: ts_CPHY_TrChRel LINE 2
- Message Structure:
CPHY_TrCH_Release_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 4
- Constraint:
ca_PHY_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 04

- No.: 4480
- Timestamp: 20:49:09:110_0
- RFN: 4115
- Chip: 25856
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 2
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 02

- No.: 4484
- Timestamp: 20:49:09:116_0
- RFN: 4116
- Chip: 11776
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 2
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 02

- No.: 4487
- Timestamp: 20:49:09:118_0
- RFN: 4116
- Chip: 21760
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 1
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 01

- No.: 4491
- Timestamp: 20:49:09:124_0
- RFN: 4117
- Chip: 4608
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 1
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 01

- No.: 4494
- Timestamp: 20:49:09:127_0
- RFN: 4117
- Chip: 15104
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 4
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 04

- No.: 4498
- Timestamp: 20:49:09:134_0
- RFN: 4118
- Chip: 3840
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 4
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 04

- No.: 4501
- Timestamp: 20:49:09:136_0
- RFN: 4118
- Chip: 14336
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 0
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 00

- No.: 4505
- Timestamp: 20:49:09:142_0
- RFN: 4118
- Chip: 35072
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity = 0
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 00

- No.: 4522
- Timestamp: 20:49:09:159_0
- RFN: 4120
- Chip: 23552
- Event: Log
- PCO: VERDICT
- Message: PASS
- Source: tc_7_2_3_18 LINE 7
- Message Structure:
no details available
- Constraint:
- BinaryMessage: