| NAS_wk34-tc_12_4_1_2ps_2004-09-13_17.39.19

TTCN Assignment: tcv_CellInfoA :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 100,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 1,
      nmo: '00'O,
      ura_Identity: '0000000000000001'B,
      t3212: '1E'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NotConfigured,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 0,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_CellInfoB :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 150,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 1,
      nmo: '00'O,
      ura_Identity: '0000000000000001'B,
      t3212: '1E'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NotConfigured,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 1000,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_CellInfoC :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 2,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 200,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 1,
      nmo: '00'O,
      ura_Identity: '0000000000000010'B,
      t3212: '1E'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NotConfigured,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 2000,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_CellInfoD :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10837
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 250,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 321,
      sfnOffset: 3000,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 1,
      nmo: '00'O,
      ura_Identity: '0000000000000010'B,
      t3212: '1E'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NotConfigured,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 3000,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_CellInfoE :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 4,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10837
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 300,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 833,
      sfnOffset: 3000,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 1,
      nmo: '00'O,
      ura_Identity: '0000000000000011'B,
      t3212: '1E'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NotConfigured,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 4000,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_CellInfoF :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 5,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10837
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 350,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 6577,
      sfnOffset: 678,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 1,
      nmo: '00'O,
      ura_Identity: '0000000000000011'B,
      t3212: '1E'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NotConfigured,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 5000,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_CellInfoG :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 6,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 400,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 7253,
      sfnOffset: 1356,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 1,
      nmo: '00'O,
      ura_Identity: '0000000000000100'B,
      t3212: '1E'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NotConfigured,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 6000,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_CellInfoH :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 7,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 450,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 4351,
      sfnOffset: 2034,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 1,
      nmo: '00'O,
      ura_Identity: '0000000000000100'B,
      t3212: '1E'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NotConfigured,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 7000,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 100,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 1,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '1E'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NotConfigured,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 0,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_CellInfoA :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 100,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 1,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '1E'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NotConfigured,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 0,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 100,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 1,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '1E'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NotConfigured,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 0,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 100,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 1,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '1E'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NotConfigured,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 0,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 100,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 1,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '1E'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NotConfigured,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 0,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 100,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 1,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '1E'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NotConfigured,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 0,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_CellInfoA :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 100,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 1,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '1E'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB_NoConn,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 0,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 100,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 1,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '1E'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB_NoConn,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 0,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_SIB3 :=

(To search, click here and then press Ctrl+F)

    {
      sib4indicator: GcTRUE,
      cellIdentity: '0000000000000000000000000000'B,
      cellSelectReselectInfo:
      {
        mappingInfo: OMIT,
        cellSelectQualityMeasure:
        [
          cpich_RSCP: NULL
        ],
        modeSpecificInfo:
        [
          fdd:
          {
            s_Intrasearch: 8,
            s_Intersearch: 8,
            s_SearchHCS: OMIT,
            rat_List:
            [
              {
                rat_Identifier: gsm,
                s_SearchRAT: -16,
                s_HCS_RAT: OMIT,
                s_Limit_SearchRAT: 0
              }
            ],
            q_QualMin: -24,
            q_RxlevMin: -40
          }
        ],
        q_Hyst_l_S: 2,
        t_Reselection_S: 0,
        hcs_ServingCellInformation: OMIT,
        maxAllowedUL_TX_Power: 21
      },
      cellAccessRestriction:
      {
        cellBarred:
        [
          notBarred: NULL
        ],
        cellReservedForOperatorUse: notReserved,
        cellReservationExtension: notReserved,
        accessClassBarredList:
        [
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred
        ]
      },
      nonCriticalExtensions: OMIT
    }

TTCN Assignment: tcv_SIB4 :=

(To search, click here and then press Ctrl+F)

    {
      cellIdentity: '0000000000000000000000000000'B,
      cellSelectReselectInfo:
      {
        mappingInfo: OMIT,
        cellSelectQualityMeasure:
        [
          cpich_RSCP: NULL
        ],
        modeSpecificInfo:
        [
          fdd:
          {
            s_Intrasearch: 8,
            s_Intersearch: 8,
            s_SearchHCS: OMIT,
            rat_List:
            [
              {
                rat_Identifier: gsm,
                s_SearchRAT: -16,
                s_HCS_RAT: OMIT,
                s_Limit_SearchRAT: 0
              }
            ],
            q_QualMin: -24,
            q_RxlevMin: -40
          }
        ],
        q_Hyst_l_S: 0,
        t_Reselection_S: 0,
        hcs_ServingCellInformation: OMIT,
        maxAllowedUL_TX_Power: 21
      },
      cellAccessRestriction:
      {
        cellBarred:
        [
          notBarred: NULL
        ],
        cellReservedForOperatorUse: notReserved,
        cellReservationExtension: notReserved,
        accessClassBarredList: OMIT
      },
      nonCriticalExtensions: OMIT
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 100,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 1,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '1E'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB_NoConn,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 0,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_SIB18 :=

(To search, click here and then press Ctrl+F)

    {
      idleModePLMNIdentities:
      {
        plmnsOfIntraFreqCellsList: OMIT,
        plmnsOfInterFreqCellsList:
        [
          {
            plmn_Identity:
            {
              mcc:
              [
                0,
                0,
                2
              ],
              mnc:
              [
                0,
                1
              ]
            }
          }
        ],
        plmnsOfInterRATCellsList: OMIT
      },
      connectedModePLMNIdentities: OMIT,
      nonCriticalExtensions: OMIT
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 100,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 1,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '1E'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB_NoConn,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 0,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_SIB11 :=

(To search, click here and then press Ctrl+F)

    {
      sib12indicator: GcTRUE,
      fach_MeasurementOccasionInfo: OMIT,
      measurementControlSysInfo:
      {
        use_of_HCS:
        [
          hcs_not_used:
          {
            cellSelectQualityMeasure:
            [
              cpich_RSCP:
              {
                intraFreqMeasurementSysInfo:
                {
                  intraFreqMeasurementID: OMIT,
                  intraFreqCellInfoSI_List:
                  {
                    removedIntraFreqCellList: OMIT,
                    newIntraFreqCellList:
                    [
                      {
                        intraFreqCellID: 0,
                        cellInfo:
                        {
                          cellIndividualOffset: OMIT,
                          referenceTimeDifferenceToCell: OMIT,
                          modeSpecificInfo:
                          [
                            fdd:
                            {
                              primaryCPICH_Info:
                              {
                                primaryScramblingCode: 100
                              },
                              primaryCPICH_TX_Power: OMIT,
                              readSFN_Indicator: GcFALSE,
                              tx_DiversityIndicator: GcFALSE
                            }
                          ],
                          cellSelectionReselectionInfo: OMIT
                        }
                      },

                      {
                        intraFreqCellID: 1,
                        cellInfo:
                        {
                          cellIndividualOffset: OMIT,
                          referenceTimeDifferenceToCell: OMIT,
                          modeSpecificInfo:
                          [
                            fdd:
                            {
                              primaryCPICH_Info:
                              {
                                primaryScramblingCode: 150
                              },
                              primaryCPICH_TX_Power: OMIT,
                              readSFN_Indicator: GcTRUE,
                              tx_DiversityIndicator: GcFALSE
                            }
                          ],
                          cellSelectionReselectionInfo: OMIT
                        }
                      },

                      {
                        intraFreqCellID: 2,
                        cellInfo:
                        {
                          cellIndividualOffset: OMIT,
                          referenceTimeDifferenceToCell: OMIT,
                          modeSpecificInfo:
                          [
                            fdd:
                            {
                              primaryCPICH_Info:
                              {
                                primaryScramblingCode: 200
                              },
                              primaryCPICH_TX_Power: OMIT,
                              readSFN_Indicator: GcTRUE,
                              tx_DiversityIndicator: GcFALSE
                            }
                          ],
                          cellSelectionReselectionInfo: OMIT
                        }
                      },

                      {
                        intraFreqCellID: 6,
                        cellInfo:
                        {
                          cellIndividualOffset: OMIT,
                          referenceTimeDifferenceToCell: OMIT,
                          modeSpecificInfo:
                          [
                            fdd:
                            {
                              primaryCPICH_Info:
                              {
                                primaryScramblingCode: 400
                              },
                              primaryCPICH_TX_Power: OMIT,
                              readSFN_Indicator: GcTRUE,
                              tx_DiversityIndicator: GcFALSE
                            }
                          ],
                          cellSelectionReselectionInfo: OMIT
                        }
                      },

                      {
                        intraFreqCellID: 7,
                        cellInfo:
                        {
                          cellIndividualOffset: OMIT,
                          referenceTimeDifferenceToCell: OMIT,
                          modeSpecificInfo:
                          [
                            fdd:
                            {
                              primaryCPICH_Info:
                              {
                                primaryScramblingCode: 450
                              },
                              primaryCPICH_TX_Power: OMIT,
                              readSFN_Indicator: GcTRUE,
                              tx_DiversityIndicator: GcFALSE
                            }
                          ],
                          cellSelectionReselectionInfo: OMIT
                        }
                      }
                    ]
                  },
                  intraFreqMeasQuantity:
                  {
                    filterCoefficient: OMIT,
                    modeSpecificInfo:
                    [
                      fdd:
                      {
                        intraFreqMeasQuantity_FDD: cpich_RSCP
                      }
                    ]
                  },
                  intraFreqReportingQuantityForRACH: OMIT,
                  maxReportedCellsOnRACH: OMIT,
                  reportingInfoForCellDCH:
                  {
                    intraFreqReportingQuantity:
                    {
                      activeSetReportingQuantities:
                      {
                        dummy: noReport,
                        cellIdentity_reportingIndicator: GcTRUE,
                        cellSynchronisationInfoReportingIndicator: GcFALSE,
                        modeSpecificInfo:
                        [
                          fdd:
                          {
                            cpich_Ec_N0_reportingIndicator: GcFALSE,
                            cpich_RSCP_reportingIndicator: GcTRUE,
                            pathloss_reportingIndicator: GcFALSE
                          }
                        ]
                      },
                      monitoredSetReportingQuantities:
                      {
                        dummy: noReport,
                        cellIdentity_reportingIndicator: GcTRUE,
                        cellSynchronisationInfoReportingIndicator: GcTRUE,
                        modeSpecificInfo:
                        [
                          fdd:
                          {
                            cpich_Ec_N0_reportingIndicator: GcFALSE,
                            cpich_RSCP_reportingIndicator: GcTRUE,
                            pathloss_reportingIndicator: GcFALSE
                          }
                        ]
                      },
                      detectedSetReportingQuantities: OMIT
                    },
                    measurementReportingMode:
                    {
                      measurementReportTransferMode: acknowledgedModeRLC,
                      periodicalOrEventTrigger: eventTrigger
                    },
                    reportCriteria:
                    [
                      intraFreqReportingCriteria:
                      {
                        eventCriteriaList:
                        [
                          {
                            event:
                            [
                              e1a:
                              {
                                triggeringCondition: monitoredSetCellsOnly,
                                reportingRange: 5,
                                forbiddenAffectCellList: OMIT,
                                w: 1,
                                reportDeactivationThreshold: t2,
                                reportingAmount: ra4,
                                reportingInterval: ri4
                              }
                            ],
                            hysteresis: 0,
                            timeToTrigger: ttt640,
                            reportingCellStatus:
                            [
                              withinActiveAndOrMonitoredUsedFreq: e3
                            ]
                          },

                          {
                            event:
                            [
                              e1b:
                              {
                                triggeringCondition: activeSetCellsOnly,
                                reportingRange: 5,
                                forbiddenAffectCellList: OMIT,
                                w: 1
                              }
                            ],
                            hysteresis: 0,
                            timeToTrigger: ttt640,
                            reportingCellStatus:
                            [
                              withinActiveAndOrMonitoredUsedFreq: e3
                            ]
                          },

                          {
                            event:
                            [
                              e1c:
                              {
                                replacementActivationThreshold: t3,
                                reportingAmount: ra4,
                                reportingInterval: ri4
                              }
                            ],
                            hysteresis: 0,
                            timeToTrigger: ttt640,
                            reportingCellStatus:
                            [
                              withinActiveAndOrMonitoredUsedFreq: e3
                            ]
                          }
                        ]
                      }
                    ]
                  }
                },
                interFreqMeasurementSysInfo:
                {
                  interFreqCellInfoSI_List:
                  {
                    removedInterFreqCellList: OMIT,
                    newInterFreqCellList:
                    [
                      {
                        interFreqCellID: 3,
                        frequencyInfo:
                        {
                          modeSpecificInfo:
                          [
                            fdd:
                            {
                              uarfcn_UL: OMIT,
                              uarfcn_DL: 10837
                            }
                          ]
                        },
                        cellInfo:
                        {
                          cellIndividualOffset: OMIT,
                          referenceTimeDifferenceToCell: OMIT,
                          modeSpecificInfo:
                          [
                            fdd:
                            {
                              primaryCPICH_Info:
                              {
                                primaryScramblingCode: 250
                              },
                              primaryCPICH_TX_Power: OMIT,
                              readSFN_Indicator: GcFALSE,
                              tx_DiversityIndicator: GcFALSE
                            }
                          ],
                          cellSelectionReselectionInfo: OMIT
                        }
                      },

                      {
                        interFreqCellID: 4,
                        frequencyInfo: OMIT,
                        cellInfo:
                        {
                          cellIndividualOffset: OMIT,
                          referenceTimeDifferenceToCell: OMIT,
                          modeSpecificInfo:
                          [
                            fdd:
                            {
                              primaryCPICH_Info:
                              {
                                primaryScramblingCode: 300
                              },
                              primaryCPICH_TX_Power: OMIT,
                              readSFN_Indicator: GcFALSE,
                              tx_DiversityIndicator: GcFALSE
                            }
                          ],
                          cellSelectionReselectionInfo: OMIT
                        }
                      },

                      {
                        interFreqCellID: 5,
                        frequencyInfo: OMIT,
                        cellInfo:
                        {
                          cellIndividualOffset: OMIT,
                          referenceTimeDifferenceToCell: OMIT,
                          modeSpecificInfo:
                          [
                            fdd:
                            {
                              primaryCPICH_Info:
                              {
                                primaryScramblingCode: 350
                              },
                              primaryCPICH_TX_Power: OMIT,
                              readSFN_Indicator: GcFALSE,
                              tx_DiversityIndicator: GcFALSE
                            }
                          ],
                          cellSelectionReselectionInfo: OMIT
                        }
                      }
                    ]
                  }
                }
              }
            ],
            interRATMeasurementSysInfo: OMIT
          }
        ],
        trafficVolumeMeasSysInfo: OMIT,
        dummy: OMIT
      },
      nonCriticalExtensions: OMIT
    }

TTCN Assignment: tcv_SIB12 :=

(To search, click here and then press Ctrl+F)

    {
      fach_MeasurementOccasionInfo: OMIT,
      measurementControlSysInfo:
      {
        use_of_HCS:
        [
          hcs_not_used:
          {
            cellSelectQualityMeasure:
            [
              cpich_RSCP:
              {
                intraFreqMeasurementSysInfo: OMIT,
                interFreqMeasurementSysInfo: OMIT
              }
            ],
            interRATMeasurementSysInfo: OMIT
          }
        ],
        trafficVolumeMeasSysInfo: OMIT,
        dummy: OMIT
      },
      nonCriticalExtensions: OMIT
    }

TTCN Assignment: tcv_SIB1 :=

(To search, click here and then press Ctrl+F)

    {
      cn_CommonGSM_MAP_NAS_SysInfo: '0001'O,
      cn_DomainSysInfoList:
      [
        {
          cn_DomainIdentity: ps_domain,
          cn_Type:
          [
            gsm_MAP: '0501'O
          ],
          cn_DRX_CycleLengthCoeff: 7
        },

        {
          cn_DomainIdentity: cs_domain,
          cn_Type:
          [
            gsm_MAP: '1E01'O
          ],
          cn_DRX_CycleLengthCoeff: 7
        }
      ],
      ue_ConnTimersAndConstants:
      {
        t_301: OMIT,
        n_301: OMIT,
        t_302: OMIT,
        n_302: OMIT,
        t_304: OMIT,
        n_304: OMIT,
        t_305: OMIT,
        t_307: OMIT,
        t_308: OMIT,
        t_309: OMIT,
        t_310: OMIT,
        n_310: OMIT,
        t_311: OMIT,
        t_312: OMIT,
        n_312: OMIT,
        t_313: OMIT,
        n_313: OMIT,
        t_314: OMIT,
        t_315: OMIT,
        n_315: OMIT,
        t_316: OMIT,
        t_317: OMIT
      },
      ue_IdleTimersAndConstants:
      {
        t_300: ms4000,
        n_300: 3,
        t_312: 10,
        n_312: s1
      },
      v3a0NonCriticalExtensions: OMIT
    }

TTCN Assignment: seg1 :=

(To search, click here and then press Ctrl+F)

    '1100010000000000000001011000100000101000000010100001000111100000000101000000000000000000000011000111010000'B

TTCN Assignment: seg2 :=

(To search, click here and then press Ctrl+F)

    '1100010000000000000001011000100000101000000010100001000111100000000101000000000000000000000011000111010000'B

TTCN Assignment: tcv_SIB3 :=

(To search, click here and then press Ctrl+F)

    {
      sib4indicator: GcTRUE,
      cellIdentity: '0000000000000000000000000000'B,
      cellSelectReselectInfo:
      {
        mappingInfo: OMIT,
        cellSelectQualityMeasure:
        [
          cpich_RSCP: NULL
        ],
        modeSpecificInfo:
        [
          fdd:
          {
            s_Intrasearch: 8,
            s_Intersearch: 8,
            s_SearchHCS: OMIT,
            rat_List:
            [
              {
                rat_Identifier: gsm,
                s_SearchRAT: -16,
                s_HCS_RAT: OMIT,
                s_Limit_SearchRAT: 0
              }
            ],
            q_QualMin: -24,
            q_RxlevMin: -40
          }
        ],
        q_Hyst_l_S: 2,
        t_Reselection_S: 0,
        hcs_ServingCellInformation: OMIT,
        maxAllowedUL_TX_Power: 21
      },
      cellAccessRestriction:
      {
        cellBarred:
        [
          notBarred: NULL
        ],
        cellReservedForOperatorUse: notReserved,
        cellReservationExtension: notReserved,
        accessClassBarredList:
        [
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred
        ]
      },
      nonCriticalExtensions: OMIT
    }

TTCN Assignment: seg1 :=

(To search, click here and then press Ctrl+F)

    '0100000000000000000000000000000010110111000110000000000000010000000000100100001000000100011111111111111111111111'B

TTCN Assignment: tcv_SIB4 :=

(To search, click here and then press Ctrl+F)

    {
      cellIdentity: '0000000000000000000000000000'B,
      cellSelectReselectInfo:
      {
        mappingInfo: OMIT,
        cellSelectQualityMeasure:
        [
          cpich_RSCP: NULL
        ],
        modeSpecificInfo:
        [
          fdd:
          {
            s_Intrasearch: 8,
            s_Intersearch: 8,
            s_SearchHCS: OMIT,
            rat_List:
            [
              {
                rat_Identifier: gsm,
                s_SearchRAT: -16,
                s_HCS_RAT: OMIT,
                s_Limit_SearchRAT: 0
              }
            ],
            q_QualMin: -24,
            q_RxlevMin: -40
          }
        ],
        q_Hyst_l_S: 0,
        t_Reselection_S: 0,
        hcs_ServingCellInformation: OMIT,
        maxAllowedUL_TX_Power: 21
      },
      cellAccessRestriction:
      {
        cellBarred:
        [
          notBarred: NULL
        ],
        cellReservedForOperatorUse: notReserved,
        cellReservationExtension: notReserved,
        accessClassBarredList: OMIT
      },
      nonCriticalExtensions: OMIT
    }

TTCN Assignment: seg1 :=

(To search, click here and then press Ctrl+F)

    '00000000000000000000000000000001011011100011000000000000001000000000010010000000000010001110111'B

TTCN Assignment: tcv_Segs :=

(To search, click here and then press Ctrl+F)

    {
      segCount: 3,
      seg1: '000101010100010000111110000000001111111101000011111111111111110111010010000100001111000000101001000011000000101010100101010110000000000000001100110001011011010101111110001010111010000011111110100000111111101000001111111010'B,
      seg2: '000011111111010000000000000000001101011000110100010000111111010011100101000001100001000011001010000000110000001110000001000000010110000010000000111000000000100010000110010000101001100100001010000000000011000000010001000101'B,
      seg3: '1100101011010110100000000000011110001000011000000001011011011011011000100000000001000011000010001001010000001011011010000000010000'B,
      seg4: OMIT,
      seg5: OMIT,
      seg6: OMIT,
      seg7: OMIT,
      seg8: OMIT,
      seg9: OMIT,
      seg10: OMIT,
      seg11: OMIT,
      seg12: OMIT,
      seg13: OMIT,
      seg14: OMIT,
      seg15: OMIT,
      seg16: OMIT
    }

TTCN Assignment: scheduling :=

(To search, click here and then press Ctrl+F)

    {
      scheduling:
      {
        segCount: 3,
        sib_Pos:
        [
          rep64: 19
        ],
        sib_PosOffsetInfo:
        [
          so4,
          so2
        ]
      }
    }

TTCN Assignment: tcv_Segs :=

(To search, click here and then press Ctrl+F)

    {
      segCount: 1,
      seg1: '0000001010010001'B,
      seg2: OMIT,
      seg3: OMIT,
      seg4: OMIT,
      seg5: OMIT,
      seg6: OMIT,
      seg7: OMIT,
      seg8: OMIT,
      seg9: OMIT,
      seg10: OMIT,
      seg11: OMIT,
      seg12: OMIT,
      seg13: OMIT,
      seg14: OMIT,
      seg15: OMIT,
      seg16: OMIT
    }

TTCN Assignment: tcv_Segs :=

(To search, click here and then press Ctrl+F)

    {
      segCount: 1,
      seg1: '100000101000000010000001'B,
      seg2: OMIT,
      seg3: OMIT,
      seg4: OMIT,
      seg5: OMIT,
      seg6: OMIT,
      seg7: OMIT,
      seg8: OMIT,
      seg9: OMIT,
      seg10: OMIT,
      seg11: OMIT,
      seg12: OMIT,
      seg13: OMIT,
      seg14: OMIT,
      seg15: OMIT,
      seg16: OMIT
    }

TTCN Assignment: tcv_SIB7 :=

(To search, click here and then press Ctrl+F)

    {
      modeSpecificInfo:
      [
        fdd:
        {
          ul_Interference: -100
        }
      ],
      prach_Information_SIB5_List:
      [
        2
      ],
      prach_Information_SIB6_List:
      [
        2
      ],
      expirationTimeFactor: OMIT,
      nonCriticalExtensions: OMIT
    }

TTCN Assignment: seg2 :=

(To search, click here and then press Ctrl+F)

    '0100000000000000000000000000000010110111000110000000000000010000000000100100001000000100011111111111111111111111'B

TTCN Assignment: seg2 :=

(To search, click here and then press Ctrl+F)

    '00000000000000000000000000000001011011100011000000000000001000000000010010000000000010001110111'B

TTCN Assignment: tcv_Segs :=

(To search, click here and then press Ctrl+F)

    {
      segCount: 2,
      seg1: '001000001101100100010010000000001000110010000100001000010010010110101000100000100110010001010011000001011001000010100111000010111000010100001000100010001100100101010100000001001010000101001010100001100001001010001000001010'B,
      seg2: '000100001100001001010010011010101000011000010010101000101100011001010100101010100001001111101000100010000001010010110000100010100001010101111000'B,
      seg3: OMIT,
      seg4: OMIT,
      seg5: OMIT,
      seg6: OMIT,
      seg7: OMIT,
      seg8: OMIT,
      seg9: OMIT,
      seg10: OMIT,
      seg11: OMIT,
      seg12: OMIT,
      seg13: OMIT,
      seg14: OMIT,
      seg15: OMIT,
      seg16: OMIT
    }

TTCN Assignment: scheduling :=

(To search, click here and then press Ctrl+F)

    {
      scheduling:
      {
        segCount: 2,
        sib_Pos:
        [
          rep64: 29
        ],
        sib_PosOffsetInfo:
        [
          so2
        ]
      }
    }

TTCN Assignment: tcv_Segs :=

(To search, click here and then press Ctrl+F)

    {
      segCount: 1,
      seg1: '000000000'B,
      seg2: OMIT,
      seg3: OMIT,
      seg4: OMIT,
      seg5: OMIT,
      seg6: OMIT,
      seg7: OMIT,
      seg8: OMIT,
      seg9: OMIT,
      seg10: OMIT,
      seg11: OMIT,
      seg12: OMIT,
      seg13: OMIT,
      seg14: OMIT,
      seg15: OMIT,
      seg16: OMIT
    }

TTCN Assignment: tcv_SIB18 :=

(To search, click here and then press Ctrl+F)

    {
      idleModePLMNIdentities:
      {
        plmnsOfIntraFreqCellsList: OMIT,
        plmnsOfInterFreqCellsList:
        [
          {
            plmn_Identity:
            {
              mcc:
              [
                0,
                0,
                2
              ],
              mnc:
              [
                0,
                1
              ]
            }
          }
        ],
        plmnsOfInterRATCellsList: OMIT
      },
      connectedModePLMNIdentities: OMIT,
      nonCriticalExtensions: OMIT
    }

TTCN Assignment: tcv_Segs :=

(To search, click here and then press Ctrl+F)

    {
      segCount: 1,
      seg1: '00010000101010001000001100110000010010010100111000101001110100000000010110100010001101110010100010010010'B,
      seg2: OMIT,
      seg3: OMIT,
      seg4: OMIT,
      seg5: OMIT,
      seg6: OMIT,
      seg7: OMIT,
      seg8: OMIT,
      seg9: OMIT,
      seg10: OMIT,
      seg11: OMIT,
      seg12: OMIT,
      seg13: OMIT,
      seg14: OMIT,
      seg15: OMIT,
      seg16: OMIT
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 100,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 1,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '1E'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB_NoConn,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 0,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_Segs :=

(To search, click here and then press Ctrl+F)

    {
      segCount: 1,
      seg1: '0000000000000000010000000010010110101010000100010000000000001000100010110000101000100010110001001000100010100001101000100110100010001110010010010011000100010000'B,
      seg2: OMIT,
      seg3: OMIT,
      seg4: OMIT,
      seg5: OMIT,
      seg6: OMIT,
      seg7: OMIT,
      seg8: OMIT,
      seg9: OMIT,
      seg10: OMIT,
      seg11: OMIT,
      seg12: OMIT,
      seg13: OMIT,
      seg14: OMIT,
      seg15: OMIT,
      seg16: OMIT
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 30,
      priScrmCode: 150,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '02'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NotConfigured,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 1000,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_CellInfoB :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 30,
      priScrmCode: 150,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '02'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NotConfigured,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 1000,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 30,
      priScrmCode: 150,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '02'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NotConfigured,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 1000,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 30,
      priScrmCode: 150,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '02'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NotConfigured,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 1000,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 30,
      priScrmCode: 150,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '02'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NotConfigured,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 1000,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 30,
      priScrmCode: 150,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '02'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NotConfigured,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 1000,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_CellInfoB :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 30,
      priScrmCode: 150,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '02'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NoDPCH,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 1000,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 30,
      priScrmCode: 150,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '02'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NoDPCH,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 1000,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_SIB3 :=

(To search, click here and then press Ctrl+F)

    {
      sib4indicator: GcTRUE,
      cellIdentity: '0000000000000000000000000001'B,
      cellSelectReselectInfo:
      {
        mappingInfo: OMIT,
        cellSelectQualityMeasure:
        [
          cpich_RSCP: NULL
        ],
        modeSpecificInfo:
        [
          fdd:
          {
            s_Intrasearch: 8,
            s_Intersearch: 8,
            s_SearchHCS: OMIT,
            rat_List:
            [
              {
                rat_Identifier: gsm,
                s_SearchRAT: -16,
                s_HCS_RAT: OMIT,
                s_Limit_SearchRAT: 0
              }
            ],
            q_QualMin: -24,
            q_RxlevMin: -40
          }
        ],
        q_Hyst_l_S: 2,
        t_Reselection_S: 0,
        hcs_ServingCellInformation: OMIT,
        maxAllowedUL_TX_Power: 21
      },
      cellAccessRestriction:
      {
        cellBarred:
        [
          notBarred: NULL
        ],
        cellReservedForOperatorUse: notReserved,
        cellReservationExtension: notReserved,
        accessClassBarredList:
        [
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred
        ]
      },
      nonCriticalExtensions: OMIT
    }

TTCN Assignment: tcv_SIB4 :=

(To search, click here and then press Ctrl+F)

    {
      cellIdentity: '0000000000000000000000000001'B,
      cellSelectReselectInfo:
      {
        mappingInfo: OMIT,
        cellSelectQualityMeasure:
        [
          cpich_RSCP: NULL
        ],
        modeSpecificInfo:
        [
          fdd:
          {
            s_Intrasearch: 8,
            s_Intersearch: 8,
            s_SearchHCS: OMIT,
            rat_List:
            [
              {
                rat_Identifier: gsm,
                s_SearchRAT: -16,
                s_HCS_RAT: OMIT,
                s_Limit_SearchRAT: 0
              }
            ],
            q_QualMin: -24,
            q_RxlevMin: -40
          }
        ],
        q_Hyst_l_S: 0,
        t_Reselection_S: 0,
        hcs_ServingCellInformation: OMIT,
        maxAllowedUL_TX_Power: 21
      },
      cellAccessRestriction:
      {
        cellBarred:
        [
          notBarred: NULL
        ],
        cellReservedForOperatorUse: notReserved,
        cellReservationExtension: notReserved,
        accessClassBarredList: OMIT
      },
      nonCriticalExtensions: OMIT
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 30,
      priScrmCode: 150,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '02'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NoDPCH,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 1000,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_SIB18 :=

(To search, click here and then press Ctrl+F)

    {
      idleModePLMNIdentities:
      {
        plmnsOfIntraFreqCellsList: OMIT,
        plmnsOfInterFreqCellsList:
        [
          {
            plmn_Identity:
            {
              mcc:
              [
                0,
                0,
                2
              ],
              mnc:
              [
                0,
                1
              ]
            }
          }
        ],
        plmnsOfInterRATCellsList: OMIT
      },
      connectedModePLMNIdentities: OMIT,
      nonCriticalExtensions: OMIT
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 30,
      priScrmCode: 150,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '02'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NoDPCH,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 1000,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_SIB11 :=

(To search, click here and then press Ctrl+F)

    {
      sib12indicator: GcTRUE,
      fach_MeasurementOccasionInfo: OMIT,
      measurementControlSysInfo:
      {
        use_of_HCS:
        [
          hcs_not_used:
          {
            cellSelectQualityMeasure:
            [
              cpich_RSCP:
              {
                intraFreqMeasurementSysInfo:
                {
                  intraFreqMeasurementID: OMIT,
                  intraFreqCellInfoSI_List:
                  {
                    removedIntraFreqCellList: OMIT,
                    newIntraFreqCellList:
                    [
                      {
                        intraFreqCellID: 1,
                        cellInfo:
                        {
                          cellIndividualOffset: OMIT,
                          referenceTimeDifferenceToCell: OMIT,
                          modeSpecificInfo:
                          [
                            fdd:
                            {
                              primaryCPICH_Info:
                              {
                                primaryScramblingCode: 150
                              },
                              primaryCPICH_TX_Power: OMIT,
                              readSFN_Indicator: GcFALSE,
                              tx_DiversityIndicator: GcFALSE
                            }
                          ],
                          cellSelectionReselectionInfo: OMIT
                        }
                      },

                      {
                        intraFreqCellID: 0,
                        cellInfo:
                        {
                          cellIndividualOffset: OMIT,
                          referenceTimeDifferenceToCell: OMIT,
                          modeSpecificInfo:
                          [
                            fdd:
                            {
                              primaryCPICH_Info:
                              {
                                primaryScramblingCode: 100
                              },
                              primaryCPICH_TX_Power: OMIT,
                              readSFN_Indicator: GcTRUE,
                              tx_DiversityIndicator: GcFALSE
                            }
                          ],
                          cellSelectionReselectionInfo: OMIT
                        }
                      },

                      {
                        intraFreqCellID: 2,
                        cellInfo:
                        {
                          cellIndividualOffset: OMIT,
                          referenceTimeDifferenceToCell: OMIT,
                          modeSpecificInfo:
                          [
                            fdd:
                            {
                              primaryCPICH_Info:
                              {
                                primaryScramblingCode: 200
                              },
                              primaryCPICH_TX_Power: OMIT,
                              readSFN_Indicator: GcTRUE,
                              tx_DiversityIndicator: GcFALSE
                            }
                          ],
                          cellSelectionReselectionInfo: OMIT
                        }
                      },

                      {
                        intraFreqCellID: 6,
                        cellInfo:
                        {
                          cellIndividualOffset: OMIT,
                          referenceTimeDifferenceToCell: OMIT,
                          modeSpecificInfo:
                          [
                            fdd:
                            {
                              primaryCPICH_Info:
                              {
                                primaryScramblingCode: 400
                              },
                              primaryCPICH_TX_Power: OMIT,
                              readSFN_Indicator: GcTRUE,
                              tx_DiversityIndicator: GcFALSE
                            }
                          ],
                          cellSelectionReselectionInfo: OMIT
                        }
                      },

                      {
                        intraFreqCellID: 7,
                        cellInfo:
                        {
                          cellIndividualOffset: OMIT,
                          referenceTimeDifferenceToCell: OMIT,
                          modeSpecificInfo:
                          [
                            fdd:
                            {
                              primaryCPICH_Info:
                              {
                                primaryScramblingCode: 450
                              },
                              primaryCPICH_TX_Power: OMIT,
                              readSFN_Indicator: GcTRUE,
                              tx_DiversityIndicator: GcFALSE
                            }
                          ],
                          cellSelectionReselectionInfo: OMIT
                        }
                      }
                    ]
                  },
                  intraFreqMeasQuantity:
                  {
                    filterCoefficient: OMIT,
                    modeSpecificInfo:
                    [
                      fdd:
                      {
                        intraFreqMeasQuantity_FDD: cpich_RSCP
                      }
                    ]
                  },
                  intraFreqReportingQuantityForRACH: OMIT,
                  maxReportedCellsOnRACH: OMIT,
                  reportingInfoForCellDCH:
                  {
                    intraFreqReportingQuantity:
                    {
                      activeSetReportingQuantities:
                      {
                        dummy: noReport,
                        cellIdentity_reportingIndicator: GcTRUE,
                        cellSynchronisationInfoReportingIndicator: GcFALSE,
                        modeSpecificInfo:
                        [
                          fdd:
                          {
                            cpich_Ec_N0_reportingIndicator: GcFALSE,
                            cpich_RSCP_reportingIndicator: GcTRUE,
                            pathloss_reportingIndicator: GcFALSE
                          }
                        ]
                      },
                      monitoredSetReportingQuantities:
                      {
                        dummy: noReport,
                        cellIdentity_reportingIndicator: GcTRUE,
                        cellSynchronisationInfoReportingIndicator: GcTRUE,
                        modeSpecificInfo:
                        [
                          fdd:
                          {
                            cpich_Ec_N0_reportingIndicator: GcFALSE,
                            cpich_RSCP_reportingIndicator: GcTRUE,
                            pathloss_reportingIndicator: GcFALSE
                          }
                        ]
                      },
                      detectedSetReportingQuantities: OMIT
                    },
                    measurementReportingMode:
                    {
                      measurementReportTransferMode: acknowledgedModeRLC,
                      periodicalOrEventTrigger: eventTrigger
                    },
                    reportCriteria:
                    [
                      intraFreqReportingCriteria:
                      {
                        eventCriteriaList:
                        [
                          {
                            event:
                            [
                              e1a:
                              {
                                triggeringCondition: monitoredSetCellsOnly,
                                reportingRange: 5,
                                forbiddenAffectCellList: OMIT,
                                w: 1,
                                reportDeactivationThreshold: t2,
                                reportingAmount: ra4,
                                reportingInterval: ri4
                              }
                            ],
                            hysteresis: 0,
                            timeToTrigger: ttt640,
                            reportingCellStatus:
                            [
                              withinActiveAndOrMonitoredUsedFreq: e3
                            ]
                          },

                          {
                            event:
                            [
                              e1b:
                              {
                                triggeringCondition: activeSetCellsOnly,
                                reportingRange: 5,
                                forbiddenAffectCellList: OMIT,
                                w: 1
                              }
                            ],
                            hysteresis: 0,
                            timeToTrigger: ttt640,
                            reportingCellStatus:
                            [
                              withinActiveAndOrMonitoredUsedFreq: e3
                            ]
                          },

                          {
                            event:
                            [
                              e1c:
                              {
                                replacementActivationThreshold: t3,
                                reportingAmount: ra4,
                                reportingInterval: ri4
                              }
                            ],
                            hysteresis: 0,
                            timeToTrigger: ttt640,
                            reportingCellStatus:
                            [
                              withinActiveAndOrMonitoredUsedFreq: e3
                            ]
                          }
                        ]
                      }
                    ]
                  }
                },
                interFreqMeasurementSysInfo:
                {
                  interFreqCellInfoSI_List:
                  {
                    removedInterFreqCellList: OMIT,
                    newInterFreqCellList:
                    [
                      {
                        interFreqCellID: 3,
                        frequencyInfo:
                        {
                          modeSpecificInfo:
                          [
                            fdd:
                            {
                              uarfcn_UL: OMIT,
                              uarfcn_DL: 10837
                            }
                          ]
                        },
                        cellInfo:
                        {
                          cellIndividualOffset: OMIT,
                          referenceTimeDifferenceToCell: OMIT,
                          modeSpecificInfo:
                          [
                            fdd:
                            {
                              primaryCPICH_Info:
                              {
                                primaryScramblingCode: 250
                              },
                              primaryCPICH_TX_Power: OMIT,
                              readSFN_Indicator: GcFALSE,
                              tx_DiversityIndicator: GcFALSE
                            }
                          ],
                          cellSelectionReselectionInfo: OMIT
                        }
                      },

                      {
                        interFreqCellID: 4,
                        frequencyInfo: OMIT,
                        cellInfo:
                        {
                          cellIndividualOffset: OMIT,
                          referenceTimeDifferenceToCell: OMIT,
                          modeSpecificInfo:
                          [
                            fdd:
                            {
                              primaryCPICH_Info:
                              {
                                primaryScramblingCode: 300
                              },
                              primaryCPICH_TX_Power: OMIT,
                              readSFN_Indicator: GcFALSE,
                              tx_DiversityIndicator: GcFALSE
                            }
                          ],
                          cellSelectionReselectionInfo: OMIT
                        }
                      },

                      {
                        interFreqCellID: 5,
                        frequencyInfo: OMIT,
                        cellInfo:
                        {
                          cellIndividualOffset: OMIT,
                          referenceTimeDifferenceToCell: OMIT,
                          modeSpecificInfo:
                          [
                            fdd:
                            {
                              primaryCPICH_Info:
                              {
                                primaryScramblingCode: 350
                              },
                              primaryCPICH_TX_Power: OMIT,
                              readSFN_Indicator: GcFALSE,
                              tx_DiversityIndicator: GcFALSE
                            }
                          ],
                          cellSelectionReselectionInfo: OMIT
                        }
                      }
                    ]
                  }
                }
              }
            ],
            interRATMeasurementSysInfo: OMIT
          }
        ],
        trafficVolumeMeasSysInfo: OMIT,
        dummy: OMIT
      },
      nonCriticalExtensions: OMIT
    }

TTCN Assignment: tcv_SIB12 :=

(To search, click here and then press Ctrl+F)

    {
      fach_MeasurementOccasionInfo: OMIT,
      measurementControlSysInfo:
      {
        use_of_HCS:
        [
          hcs_not_used:
          {
            cellSelectQualityMeasure:
            [
              cpich_RSCP:
              {
                intraFreqMeasurementSysInfo: OMIT,
                interFreqMeasurementSysInfo: OMIT
              }
            ],
            interRATMeasurementSysInfo: OMIT
          }
        ],
        trafficVolumeMeasSysInfo: OMIT,
        dummy: OMIT
      },
      nonCriticalExtensions: OMIT
    }

TTCN Assignment: tcv_SIB1 :=

(To search, click here and then press Ctrl+F)

    {
      cn_CommonGSM_MAP_NAS_SysInfo: '0001'O,
      cn_DomainSysInfoList:
      [
        {
          cn_DomainIdentity: ps_domain,
          cn_Type:
          [
            gsm_MAP: '0201'O
          ],
          cn_DRX_CycleLengthCoeff: 7
        },

        {
          cn_DomainIdentity: cs_domain,
          cn_Type:
          [
            gsm_MAP: '0000'O
          ],
          cn_DRX_CycleLengthCoeff: 7
        }
      ],
      ue_ConnTimersAndConstants:
      {
        t_301: OMIT,
        n_301: OMIT,
        t_302: OMIT,
        n_302: OMIT,
        t_304: OMIT,
        n_304: OMIT,
        t_305: OMIT,
        t_307: OMIT,
        t_308: OMIT,
        t_309: OMIT,
        t_310: OMIT,
        n_310: OMIT,
        t_311: OMIT,
        t_312: OMIT,
        n_312: OMIT,
        t_313: OMIT,
        n_313: OMIT,
        t_314: OMIT,
        t_315: OMIT,
        n_315: OMIT,
        t_316: OMIT,
        t_317: OMIT
      },
      ue_IdleTimersAndConstants:
      {
        t_300: ms4000,
        n_300: 3,
        t_312: 10,
        n_312: s1
      },
      v3a0NonCriticalExtensions: OMIT
    }

TTCN Assignment: seg1 :=

(To search, click here and then press Ctrl+F)

    '1100010000000000000001011000100000010000000010100001000000000000000001000000000000000000000011000111010000'B

TTCN Assignment: seg2 :=

(To search, click here and then press Ctrl+F)

    '1100010000000000000001011000100000010000000010100001000000000000000001000000000000000000000011000111010000'B

TTCN Assignment: tcv_SIB3 :=

(To search, click here and then press Ctrl+F)

    {
      sib4indicator: GcTRUE,
      cellIdentity: '0000000000000000000000000001'B,
      cellSelectReselectInfo:
      {
        mappingInfo: OMIT,
        cellSelectQualityMeasure:
        [
          cpich_RSCP: NULL
        ],
        modeSpecificInfo:
        [
          fdd:
          {
            s_Intrasearch: 8,
            s_Intersearch: 8,
            s_SearchHCS: OMIT,
            rat_List:
            [
              {
                rat_Identifier: gsm,
                s_SearchRAT: -16,
                s_HCS_RAT: OMIT,
                s_Limit_SearchRAT: 0
              }
            ],
            q_QualMin: -24,
            q_RxlevMin: -40
          }
        ],
        q_Hyst_l_S: 2,
        t_Reselection_S: 0,
        hcs_ServingCellInformation: OMIT,
        maxAllowedUL_TX_Power: 21
      },
      cellAccessRestriction:
      {
        cellBarred:
        [
          notBarred: NULL
        ],
        cellReservedForOperatorUse: notReserved,
        cellReservationExtension: notReserved,
        accessClassBarredList:
        [
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred
        ]
      },
      nonCriticalExtensions: OMIT
    }

TTCN Assignment: seg1 :=

(To search, click here and then press Ctrl+F)

    '0100000000000000000000000000010010110111000110000000000000010000000000100100001000000100011111111111111111111111'B

TTCN Assignment: tcv_SIB4 :=

(To search, click here and then press Ctrl+F)

    {
      cellIdentity: '0000000000000000000000000001'B,
      cellSelectReselectInfo:
      {
        mappingInfo: OMIT,
        cellSelectQualityMeasure:
        [
          cpich_RSCP: NULL
        ],
        modeSpecificInfo:
        [
          fdd:
          {
            s_Intrasearch: 8,
            s_Intersearch: 8,
            s_SearchHCS: OMIT,
            rat_List:
            [
              {
                rat_Identifier: gsm,
                s_SearchRAT: -16,
                s_HCS_RAT: OMIT,
                s_Limit_SearchRAT: 0
              }
            ],
            q_QualMin: -24,
            q_RxlevMin: -40
          }
        ],
        q_Hyst_l_S: 0,
        t_Reselection_S: 0,
        hcs_ServingCellInformation: OMIT,
        maxAllowedUL_TX_Power: 21
      },
      cellAccessRestriction:
      {
        cellBarred:
        [
          notBarred: NULL
        ],
        cellReservedForOperatorUse: notReserved,
        cellReservationExtension: notReserved,
        accessClassBarredList: OMIT
      },
      nonCriticalExtensions: OMIT
    }

TTCN Assignment: seg1 :=

(To search, click here and then press Ctrl+F)

    '00000000000000000000000000001001011011100011000000000000001000000000010010000000000010001110111'B

TTCN Assignment: tcv_Segs :=

(To search, click here and then press Ctrl+F)

    {
      segCount: 3,
      seg1: '000101010100010000111110000000001111111101000011111111111111110111010010000100001111000000101001000011000000101010100101010110000000000000001100110001011011010101111110001010111010000011111110100000111111101000001111111010'B,
      seg2: '000011111111010000000000000000001101011000110100010000111111010011100101000001100001000011001010000000110000001110000001000000010110000010000000111000000000100010000110010000101001100100001010000000000011000000010001000101'B,
      seg3: '1100101011010110100000000000011110001000011000000001011011011011011000100000000001000011000010001001010000001011011010000000010000'B,
      seg4: OMIT,
      seg5: OMIT,
      seg6: OMIT,
      seg7: OMIT,
      seg8: OMIT,
      seg9: OMIT,
      seg10: OMIT,
      seg11: OMIT,
      seg12: OMIT,
      seg13: OMIT,
      seg14: OMIT,
      seg15: OMIT,
      seg16: OMIT
    }

TTCN Assignment: scheduling :=

(To search, click here and then press Ctrl+F)

    {
      scheduling:
      {
        segCount: 3,
        sib_Pos:
        [
          rep64: 19
        ],
        sib_PosOffsetInfo:
        [
          so4,
          so2
        ]
      }
    }

TTCN Assignment: tcv_Segs :=

(To search, click here and then press Ctrl+F)

    {
      segCount: 1,
      seg1: '0000001010010001'B,
      seg2: OMIT,
      seg3: OMIT,
      seg4: OMIT,
      seg5: OMIT,
      seg6: OMIT,
      seg7: OMIT,
      seg8: OMIT,
      seg9: OMIT,
      seg10: OMIT,
      seg11: OMIT,
      seg12: OMIT,
      seg13: OMIT,
      seg14: OMIT,
      seg15: OMIT,
      seg16: OMIT
    }

TTCN Assignment: tcv_Segs :=

(To search, click here and then press Ctrl+F)

    {
      segCount: 1,
      seg1: '100000101000000010000001'B,
      seg2: OMIT,
      seg3: OMIT,
      seg4: OMIT,
      seg5: OMIT,
      seg6: OMIT,
      seg7: OMIT,
      seg8: OMIT,
      seg9: OMIT,
      seg10: OMIT,
      seg11: OMIT,
      seg12: OMIT,
      seg13: OMIT,
      seg14: OMIT,
      seg15: OMIT,
      seg16: OMIT
    }

TTCN Assignment: tcv_SIB7 :=

(To search, click here and then press Ctrl+F)

    {
      modeSpecificInfo:
      [
        fdd:
        {
          ul_Interference: -100
        }
      ],
      prach_Information_SIB5_List:
      [
        2
      ],
      prach_Information_SIB6_List:
      [
        2
      ],
      expirationTimeFactor: OMIT,
      nonCriticalExtensions: OMIT
    }

TTCN Assignment: seg2 :=

(To search, click here and then press Ctrl+F)

    '0100000000000000000000000000010010110111000110000000000000010000000000100100001000000100011111111111111111111111'B

TTCN Assignment: seg2 :=

(To search, click here and then press Ctrl+F)

    '00000000000000000000000000001001011011100011000000000000001000000000010010000000000010001110111'B

TTCN Assignment: tcv_Segs :=

(To search, click here and then press Ctrl+F)

    {
      segCount: 2,
      seg1: '001000001101100100010010000100001001001011000100000000010001100100101000100000100110010001010011000001011001000010100111000010111000010100001000100010001100100101010100000001001010000101001010100001100001001010001000001010'B,
      seg2: '000100001100001001010010011010101000011000010010101000101100011001010100101010100001001111101000100010000001010010110000100010100001010101111000'B,
      seg3: OMIT,
      seg4: OMIT,
      seg5: OMIT,
      seg6: OMIT,
      seg7: OMIT,
      seg8: OMIT,
      seg9: OMIT,
      seg10: OMIT,
      seg11: OMIT,
      seg12: OMIT,
      seg13: OMIT,
      seg14: OMIT,
      seg15: OMIT,
      seg16: OMIT
    }

TTCN Assignment: scheduling :=

(To search, click here and then press Ctrl+F)

    {
      scheduling:
      {
        segCount: 2,
        sib_Pos:
        [
          rep64: 29
        ],
        sib_PosOffsetInfo:
        [
          so2
        ]
      }
    }

TTCN Assignment: tcv_Segs :=

(To search, click here and then press Ctrl+F)

    {
      segCount: 1,
      seg1: '000000000'B,
      seg2: OMIT,
      seg3: OMIT,
      seg4: OMIT,
      seg5: OMIT,
      seg6: OMIT,
      seg7: OMIT,
      seg8: OMIT,
      seg9: OMIT,
      seg10: OMIT,
      seg11: OMIT,
      seg12: OMIT,
      seg13: OMIT,
      seg14: OMIT,
      seg15: OMIT,
      seg16: OMIT
    }

TTCN Assignment: tcv_SIB18 :=

(To search, click here and then press Ctrl+F)

    {
      idleModePLMNIdentities:
      {
        plmnsOfIntraFreqCellsList: OMIT,
        plmnsOfInterFreqCellsList:
        [
          {
            plmn_Identity:
            {
              mcc:
              [
                0,
                0,
                2
              ],
              mnc:
              [
                0,
                1
              ]
            }
          }
        ],
        plmnsOfInterRATCellsList: OMIT
      },
      connectedModePLMNIdentities: OMIT,
      nonCriticalExtensions: OMIT
    }

TTCN Assignment: tcv_Segs :=

(To search, click here and then press Ctrl+F)

    {
      segCount: 1,
      seg1: '00010000101100001000001100110000010010010101011000101001110100000000010111000010001101110011000010010010'B,
      seg2: OMIT,
      seg3: OMIT,
      seg4: OMIT,
      seg5: OMIT,
      seg6: OMIT,
      seg7: OMIT,
      seg8: OMIT,
      seg9: OMIT,
      seg10: OMIT,
      seg11: OMIT,
      seg12: OMIT,
      seg13: OMIT,
      seg14: OMIT,
      seg15: OMIT,
      seg16: OMIT
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 30,
      priScrmCode: 150,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '02'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NoDPCH,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 1000,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_Segs :=

(To search, click here and then press Ctrl+F)

    {
      segCount: 1,
      seg1: '0001000000000000010000000010010110101100000100010000000000010000100010110000110000100010110001010000100010100001110000100110100010010110010010010011000100010000'B,
      seg2: OMIT,
      seg3: OMIT,
      seg4: OMIT,
      seg5: OMIT,
      seg6: OMIT,
      seg7: OMIT,
      seg8: OMIT,
      seg9: OMIT,
      seg10: OMIT,
      seg11: OMIT,
      seg12: OMIT,
      seg13: OMIT,
      seg14: OMIT,
      seg15: OMIT,
      seg16: OMIT
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 100,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 1,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '1E'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB_NoConn,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 0,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 100,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 1,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '1E'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB_NoConn,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 0,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 100,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 1,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '1E'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB_NoConn,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 0,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_InitialUE_Id :=

(To search, click here and then press Ctrl+F)

    [
      p_TMSI_and_RAI:
      {
        p_TMSI: '00010010001101000101011001111000'B,
        rai:
        {
          lai:
          {
            plmn_Identity:
            {
              mcc:
              [
                0,
                0,
                1
              ],
              mnc:
              [
                0,
                1
              ]
            },
            lac: '0000000000000010'B
          },
          rac: '00000101'B
        }
      }
    ]

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 100,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 1,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '1E'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB_NoConn,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 0,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_CellInfoA :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 100,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 1,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '1E'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 0,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 100,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 1,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '1E'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 0,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_StartList :=

(To search, click here and then press Ctrl+F)

    [
      {
        cn_DomainIdentity: ps_domain,
        start_Value: '00000000000000000010'B
      },

      {
        cn_DomainIdentity: cs_domain,
        start_Value: '00000000000000000010'B
      }
    ]

TTCN Assignment: tcv_AuthXDOUT :=

(To search, click here and then press Ctrl+F)

    '01010101010001000111011101100110000100010000000000110011001000101101110111001100111111111110111010011001100010001011101110101010'B

TTCN Assignment: tcv_AuthAUTN_2 :=

(To search, click here and then press Ctrl+F)

    '00000000000000000101010101000100011101110110011000010001000000000011001100100010'B

TTCN Assignment: tcv_AuthAUTN :=

(To search, click here and then press Ctrl+F)

    '01100110000100010000000000110011001000101101110100000000000000000101010101000100011101110110011000010001000000000011001100100010'B

TTCN Assignment: tcv_AuthIK :=

(To search, click here and then press Ctrl+F)

    '01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100'B

TTCN Assignment: tcv_AuthCK :=

(To search, click here and then press Ctrl+F)

    '01000100011101110110011000010001000000000011001100100010110111011100110011111111111011101001100110001000101110111010101001010101'B

TTCN Assignment: tcv_AuthXRES :=

(To search, click here and then press Ctrl+F)

    '01010101010001000111011101100110000100010000000000110011001000101101110111001100111111111110111010011001100010001011101110101010'B

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 100,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 1,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '1E'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 0,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: dL_Integrity :=

(To search, click here and then press Ctrl+F)

    {
      integrityProtectionModeCommand:
      [
        startIntegrityProtection:
        {
          integrityProtInitNumber: '00001111000011110000111100001111'B
        }
      ],
      integrityProtectionAlgorithm: uia1
    }

TTCN Assignment: dl_IntegrityCheckInfo :=

(To search, click here and then press Ctrl+F)

    {
      messageAuthenticationCode: '00000000000000000000000000000000'B,
      rrc_MessageSequenceNumber: 0
    }

TTCN Assignment: tcv_CellInfoA :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 100,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 1,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '1E'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 0,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 100,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 1,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '1E'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 0,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_AuthXDOUT :=

(To search, click here and then press Ctrl+F)

    '01010101010001000111011101100110000100010000000000110011001000101101110111001100111111111110111010011001100010001011101110101010'B

TTCN Assignment: tcv_AuthAUTN_2 :=

(To search, click here and then press Ctrl+F)

    '00000000000000000101010101000100011101110110011000010001000000000011001100100010'B

TTCN Assignment: tcv_AuthAUTN :=

(To search, click here and then press Ctrl+F)

    '01100110000100010000000000110011001000101101110100000000000000000101010101000100011101110110011000010001000000000011001100100010'B

TTCN Assignment: tcv_PS_AuthIK :=

(To search, click here and then press Ctrl+F)

    '01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100'B

TTCN Assignment: tcv_PS_AuthCK :=

(To search, click here and then press Ctrl+F)

    '01000100011101110110011000010001000000000011001100100010110111011100110011111111111011101001100110001000101110111010101001010101'B

TTCN Assignment: tcv_AuthXRES :=

(To search, click here and then press Ctrl+F)

    '01010101010001000111011101100110000100010000000000110011001000101101110111001100111111111110111010011001100010001011101110101010'B

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 100,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 1,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '1E'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 0,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: dL_Integrity :=

(To search, click here and then press Ctrl+F)

    {
      integrityProtectionModeCommand:
      [
        modify:
        {
          dl_IntegrityProtActivationInfo:
          {
            rrc_MessageSequenceNumberList:
            [
              0,
              0,
              1,
              2,
              0
            ]
          }
        }
      ],
      integrityProtectionAlgorithm: uia1
    }

TTCN Assignment: tcv_CellInfoA :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 100,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 1,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '1E'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 0,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 100,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 1,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '1E'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 0,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 100,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 1,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '1E'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 0,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 100,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 1,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '1E'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 0,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_CellInfoA :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 100,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 1,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '1E'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB_NoConn,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 0,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_CellIndInfo :=

(To search, click here and then press Ctrl+F)

    {
      cs_cipheringStarted: GcFALSE,
      ps_cipheringStarted: GcFALSE,
      recentSecureDomain: cs_domain,
      dL_CipherMode:
      [
        dummy: NULL
      ],
      uL_CipherMode: OMIT,
      cipheringAlgorithmCapability: '0000000000000011'B,
      integrityStarted: GcFALSE,
      dL_Integrity:
      {
        integrityProtectionModeCommand:
        [
          startIntegrityProtection:
          {
            integrityProtInitNumber: '00001111000011110000111100001111'B
          }
        ],
        integrityProtectionAlgorithm: uia1
      },
      uL_Integrity: OMIT,
      dl_IntegrityCheckInfo: OMIT,
      start_CS: '00000000000000000000'B,
      start_PS: '00000000000000000000'B
    }

TTCN Assignment: tcv_SIB1 :=

(To search, click here and then press Ctrl+F)

    {
      cn_CommonGSM_MAP_NAS_SysInfo: '0001'O,
      cn_DomainSysInfoList:
      [
        {
          cn_DomainIdentity: ps_domain,
          cn_Type:
          [
            gsm_MAP: '0501'O
          ],
          cn_DRX_CycleLengthCoeff: 7
        },

        {
          cn_DomainIdentity: cs_domain,
          cn_Type:
          [
            gsm_MAP: '0000'O
          ],
          cn_DRX_CycleLengthCoeff: 7
        }
      ],
      ue_ConnTimersAndConstants:
      {
        t_301: OMIT,
        n_301: OMIT,
        t_302: OMIT,
        n_302: OMIT,
        t_304: OMIT,
        n_304: OMIT,
        t_305: OMIT,
        t_307: OMIT,
        t_308: OMIT,
        t_309: OMIT,
        t_310: OMIT,
        n_310: OMIT,
        t_311: OMIT,
        t_312: OMIT,
        n_312: OMIT,
        t_313: OMIT,
        n_313: OMIT,
        t_314: OMIT,
        t_315: OMIT,
        n_315: OMIT,
        t_316: OMIT,
        t_317: OMIT
      },
      ue_IdleTimersAndConstants:
      {
        t_300: ms4000,
        n_300: 3,
        t_312: 10,
        n_312: s1
      },
      v3a0NonCriticalExtensions: OMIT
    }

TTCN Assignment: seg1 :=

(To search, click here and then press Ctrl+F)

    '1100010000000000000001011000100000101000000010100001000000000000000001000000000000000000000011000111010000'B

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 100,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB_NoConn,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 0,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_Segs :=

(To search, click here and then press Ctrl+F)

    {
      segCount: 1,
      seg1: '0010000000000000010000000010010110101100000100010000000000011000100010110000110000100010110001010000100010100001110000100110100010010110010010010011000100010000'B,
      seg2: OMIT,
      seg3: OMIT,
      seg4: OMIT,
      seg5: OMIT,
      seg6: OMIT,
      seg7: OMIT,
      seg8: OMIT,
      seg9: OMIT,
      seg10: OMIT,
      seg11: OMIT,
      seg12: OMIT,
      seg13: OMIT,
      seg14: OMIT,
      seg15: OMIT,
      seg16: OMIT
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 100,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB_NoConn,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 0,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 100,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB_NoConn,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 0,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 100,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB_NoConn,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 0,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 100,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB_NoConn,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 0,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 100,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB_NoConn,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 0,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_InitialUE_Id :=

(To search, click here and then press Ctrl+F)

    [
      tmsi_and_LAI:
      {
        tmsi: '00010001001000100011001101000100'B,
        lai:
        {
          plmn_Identity:
          {
            mcc:
            [
              0,
              0,
              1
            ],
            mnc:
            [
              0,
              1
            ]
          },
          lac: '0000000000000001'B
        }
      }
    ]

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 100,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB_NoConn,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 0,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_CellInfoA :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 100,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 0,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 100,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 0,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_StartList :=

(To search, click here and then press Ctrl+F)

    [
      {
        cn_DomainIdentity: ps_domain,
        start_Value: '00000000000000000010'B
      },

      {
        cn_DomainIdentity: cs_domain,
        start_Value: '00000000000000000010'B
      }
    ]

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 100,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 0,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 100,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 0,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_CellInfoA :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 100,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB_NoConn,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 0,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_CellIndInfo :=

(To search, click here and then press Ctrl+F)

    {
      cs_cipheringStarted: GcFALSE,
      ps_cipheringStarted: GcFALSE,
      recentSecureDomain: cs_domain,
      dL_CipherMode:
      [
        dummy: NULL
      ],
      uL_CipherMode: OMIT,
      cipheringAlgorithmCapability: '0000000000000011'B,
      integrityStarted: GcFALSE,
      dL_Integrity:
      {
        integrityProtectionModeCommand:
        [
          startIntegrityProtection:
          {
            integrityProtInitNumber: '00001111000011110000111100001111'B
          }
        ],
        integrityProtectionAlgorithm: uia1
      },
      uL_Integrity: OMIT,
      dl_IntegrityCheckInfo: OMIT,
      start_CS: '00000000000000000000'B,
      start_PS: '00000000000000000000'B
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 100,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB_NoConn,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 0,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 100,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB_NoConn,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 0,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_InitialUE_Id :=

(To search, click here and then press Ctrl+F)

    [
      tmsi_and_LAI:
      {
        tmsi: '00010001001000100011001101000100'B,
        lai:
        {
          plmn_Identity:
          {
            mcc:
            [
              0,
              0,
              1
            ],
            mnc:
            [
              0,
              1
            ]
          },
          lac: '0000000000000001'B
        }
      }
    ]

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 100,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB_NoConn,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 0,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_CellInfoA :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 100,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 0,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 100,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 0,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_StartList :=

(To search, click here and then press Ctrl+F)

    [
      {
        cn_DomainIdentity: ps_domain,
        start_Value: '00000000000000000010'B
      },

      {
        cn_DomainIdentity: cs_domain,
        start_Value: '00000000000000000010'B
      }
    ]

TTCN Assignment: tcv_AuthXDOUT :=

(To search, click here and then press Ctrl+F)

    '01010101010001000111011101100110000100010000000000110011001000101101110111001100111111111110111010011001100010001011101110101010'B

TTCN Assignment: tcv_AuthAUTN_2 :=

(To search, click here and then press Ctrl+F)

    '00000000000000000101010101000100011101110110011000010001000000000011001100100010'B

TTCN Assignment: tcv_AuthAUTN :=

(To search, click here and then press Ctrl+F)

    '01100110000100010000000000110011001000101101110100000000000000000101010101000100011101110110011000010001000000000011001100100010'B

TTCN Assignment: tcv_PS_AuthIK :=

(To search, click here and then press Ctrl+F)

    '01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100'B

TTCN Assignment: tcv_PS_AuthCK :=

(To search, click here and then press Ctrl+F)

    '01000100011101110110011000010001000000000011001100100010110111011100110011111111111011101001100110001000101110111010101001010101'B

TTCN Assignment: tcv_AuthXRES :=

(To search, click here and then press Ctrl+F)

    '01010101010001000111011101100110000100010000000000110011001000101101110111001100111111111110111010011001100010001011101110101010'B

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 100,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 0,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: dL_Integrity :=

(To search, click here and then press Ctrl+F)

    {
      integrityProtectionModeCommand:
      [
        startIntegrityProtection:
        {
          integrityProtInitNumber: '00001111000011110000111100001111'B
        }
      ],
      integrityProtectionAlgorithm: uia1
    }

TTCN Assignment: dl_IntegrityCheckInfo :=

(To search, click here and then press Ctrl+F)

    {
      messageAuthenticationCode: '00000000000000000000000000000000'B,
      rrc_MessageSequenceNumber: 0
    }

TTCN Assignment: tcv_CellInfoA :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 100,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 0,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 100,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 0,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 100,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 0,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 100,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 0,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_CellInfoA :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 100,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB_NoConn,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 0,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_CellIndInfo :=

(To search, click here and then press Ctrl+F)

    {
      cs_cipheringStarted: GcFALSE,
      ps_cipheringStarted: GcFALSE,
      recentSecureDomain: cs_domain,
      dL_CipherMode:
      [
        dummy: NULL
      ],
      uL_CipherMode: OMIT,
      cipheringAlgorithmCapability: '0000000000000011'B,
      integrityStarted: GcFALSE,
      dL_Integrity:
      {
        integrityProtectionModeCommand:
        [
          startIntegrityProtection:
          {
            integrityProtInitNumber: '00001111000011110000111100001111'B
          }
        ],
        integrityProtectionAlgorithm: uia1
      },
      uL_Integrity: OMIT,
      dl_IntegrityCheckInfo: OMIT,
      start_CS: '00000000000000000000'B,
      start_PS: '00000000000000000000'B
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 100,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB_NoConn,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 0,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 100,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB_NoConn,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 0,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_CellInfoA :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 10,
      priScrmCode: 100,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB_NoConn,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 0,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 30,
      priScrmCode: 150,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '02'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NoDPCH,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 1000,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 30,
      priScrmCode: 150,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '02'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NoDPCH,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 1000,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_CellInfoB :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 150,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '02'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NoDPCH,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 1000,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 150,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '02'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NoDPCH,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 1000,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 10,
      priScrmCode: 100,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB_NoConn,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 0,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 150,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '02'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NoDPCH,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 1000,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_CellInfoB :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 150,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '02'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB_NoConn,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 1000,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 150,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '02'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB_NoConn,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 1000,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_InitialUE_Id :=

(To search, click here and then press Ctrl+F)

    [
      tmsi_and_LAI:
      {
        tmsi: '00010001001000100011001101000100'B,
        lai:
        {
          plmn_Identity:
          {
            mcc:
            [
              0,
              0,
              1
            ],
            mnc:
            [
              0,
              1
            ]
          },
          lac: '0000000000000001'B
        }
      }
    ]

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 150,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '02'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB_NoConn,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 1000,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_CellInfoB :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 150,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '02'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 1000,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 150,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '02'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 1000,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_StartList :=

(To search, click here and then press Ctrl+F)

    [
      {
        cn_DomainIdentity: ps_domain,
        start_Value: '00000000000000000010'B
      },

      {
        cn_DomainIdentity: cs_domain,
        start_Value: '00000000000000000010'B
      }
    ]

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 150,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '02'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 1000,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 150,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '02'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 1000,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_CellInfoB :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 150,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '02'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB_NoConn,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 1000,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_CellIndInfo :=

(To search, click here and then press Ctrl+F)

    {
      cs_cipheringStarted: GcFALSE,
      ps_cipheringStarted: GcFALSE,
      recentSecureDomain: cs_domain,
      dL_CipherMode:
      [
        dummy: NULL
      ],
      uL_CipherMode: OMIT,
      cipheringAlgorithmCapability: '0000000000000011'B,
      integrityStarted: GcFALSE,
      dL_Integrity:
      {
        integrityProtectionModeCommand:
        [
          startIntegrityProtection:
          {
            integrityProtInitNumber: '00001111000011110000111100001111'B
          }
        ],
        integrityProtectionAlgorithm: uia1
      },
      uL_Integrity: OMIT,
      dl_IntegrityCheckInfo: OMIT,
      start_CS: '00000000000000000000'B,
      start_PS: '00000000000000000000'B
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 150,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '02'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB_NoConn,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 1000,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 10,
      priScrmCode: 100,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NoDPCH,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 0,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 10,
      priScrmCode: 100,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NoDPCH,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 0,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_CellInfoA :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 10,
      priScrmCode: 100,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NotConfigured,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 0,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 150,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '02'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB_NoConn,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 1000,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 150,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '02'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB_NoConn,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 1000,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_CellInfoB :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 30,
      priScrmCode: 150,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '02'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB_NoConn,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 1000,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10837
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 250,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 321,
      sfnOffset: 3000,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '002'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000010'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NotConfigured,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 3000,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_CellInfoD :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10837
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 250,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 321,
      sfnOffset: 3000,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '002'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000010'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NotConfigured,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 3000,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10837
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 250,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 321,
      sfnOffset: 3000,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '002'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000010'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NotConfigured,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 3000,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10837
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 250,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 321,
      sfnOffset: 3000,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '002'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000010'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NotConfigured,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 3000,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10837
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 250,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 321,
      sfnOffset: 3000,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '002'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000010'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NotConfigured,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 3000,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10837
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 250,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 321,
      sfnOffset: 3000,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '002'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000010'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NotConfigured,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 3000,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_CellInfoD :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10837
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 250,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 321,
      sfnOffset: 3000,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '002'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000010'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NoDPCH,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 3000,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10837
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 250,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 321,
      sfnOffset: 3000,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '002'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000010'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NoDPCH,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 3000,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_SIB3 :=

(To search, click here and then press Ctrl+F)

    {
      sib4indicator: GcTRUE,
      cellIdentity: '0000000000000000000000000011'B,
      cellSelectReselectInfo:
      {
        mappingInfo: OMIT,
        cellSelectQualityMeasure:
        [
          cpich_RSCP: NULL
        ],
        modeSpecificInfo:
        [
          fdd:
          {
            s_Intrasearch: 8,
            s_Intersearch: 8,
            s_SearchHCS: OMIT,
            rat_List:
            [
              {
                rat_Identifier: gsm,
                s_SearchRAT: -16,
                s_HCS_RAT: OMIT,
                s_Limit_SearchRAT: 0
              }
            ],
            q_QualMin: -24,
            q_RxlevMin: -40
          }
        ],
        q_Hyst_l_S: 2,
        t_Reselection_S: 0,
        hcs_ServingCellInformation: OMIT,
        maxAllowedUL_TX_Power: 21
      },
      cellAccessRestriction:
      {
        cellBarred:
        [
          notBarred: NULL
        ],
        cellReservedForOperatorUse: notReserved,
        cellReservationExtension: notReserved,
        accessClassBarredList:
        [
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred
        ]
      },
      nonCriticalExtensions: OMIT
    }

TTCN Assignment: tcv_SIB4 :=

(To search, click here and then press Ctrl+F)

    {
      cellIdentity: '0000000000000000000000000011'B,
      cellSelectReselectInfo:
      {
        mappingInfo: OMIT,
        cellSelectQualityMeasure:
        [
          cpich_RSCP: NULL
        ],
        modeSpecificInfo:
        [
          fdd:
          {
            s_Intrasearch: 8,
            s_Intersearch: 8,
            s_SearchHCS: OMIT,
            rat_List:
            [
              {
                rat_Identifier: gsm,
                s_SearchRAT: -16,
                s_HCS_RAT: OMIT,
                s_Limit_SearchRAT: 0
              }
            ],
            q_QualMin: -24,
            q_RxlevMin: -40
          }
        ],
        q_Hyst_l_S: 0,
        t_Reselection_S: 0,
        hcs_ServingCellInformation: OMIT,
        maxAllowedUL_TX_Power: 21
      },
      cellAccessRestriction:
      {
        cellBarred:
        [
          notBarred: NULL
        ],
        cellReservedForOperatorUse: notReserved,
        cellReservationExtension: notReserved,
        accessClassBarredList: OMIT
      },
      nonCriticalExtensions: OMIT
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10837
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 250,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 321,
      sfnOffset: 3000,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '002'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000010'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NoDPCH,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 3000,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_SIB18 :=

(To search, click here and then press Ctrl+F)

    {
      idleModePLMNIdentities:
      {
        plmnsOfIntraFreqCellsList: OMIT,
        plmnsOfInterFreqCellsList:
        [
          {
            plmn_Identity:
            {
              mcc:
              [
                0,
                0,
                1
              ],
              mnc:
              [
                0,
                1
              ]
            }
          }
        ],
        plmnsOfInterRATCellsList: OMIT
      },
      connectedModePLMNIdentities: OMIT,
      nonCriticalExtensions: OMIT
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10837
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 250,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 321,
      sfnOffset: 3000,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '002'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000010'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NoDPCH,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 3000,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_SIB11 :=

(To search, click here and then press Ctrl+F)

    {
      sib12indicator: GcTRUE,
      fach_MeasurementOccasionInfo: OMIT,
      measurementControlSysInfo:
      {
        use_of_HCS:
        [
          hcs_not_used:
          {
            cellSelectQualityMeasure:
            [
              cpich_RSCP:
              {
                intraFreqMeasurementSysInfo:
                {
                  intraFreqMeasurementID: OMIT,
                  intraFreqCellInfoSI_List:
                  {
                    removedIntraFreqCellList: OMIT,
                    newIntraFreqCellList:
                    [
                      {
                        intraFreqCellID: 3,
                        cellInfo:
                        {
                          cellIndividualOffset: OMIT,
                          referenceTimeDifferenceToCell: OMIT,
                          modeSpecificInfo:
                          [
                            fdd:
                            {
                              primaryCPICH_Info:
                              {
                                primaryScramblingCode: 250
                              },
                              primaryCPICH_TX_Power: OMIT,
                              readSFN_Indicator: GcFALSE,
                              tx_DiversityIndicator: GcFALSE
                            }
                          ],
                          cellSelectionReselectionInfo: OMIT
                        }
                      },

                      {
                        intraFreqCellID: 4,
                        cellInfo:
                        {
                          cellIndividualOffset: OMIT,
                          referenceTimeDifferenceToCell: OMIT,
                          modeSpecificInfo:
                          [
                            fdd:
                            {
                              primaryCPICH_Info:
                              {
                                primaryScramblingCode: 300
                              },
                              primaryCPICH_TX_Power: OMIT,
                              readSFN_Indicator: GcTRUE,
                              tx_DiversityIndicator: GcFALSE
                            }
                          ],
                          cellSelectionReselectionInfo: OMIT
                        }
                      },

                      {
                        intraFreqCellID: 5,
                        cellInfo:
                        {
                          cellIndividualOffset: OMIT,
                          referenceTimeDifferenceToCell: OMIT,
                          modeSpecificInfo:
                          [
                            fdd:
                            {
                              primaryCPICH_Info:
                              {
                                primaryScramblingCode: 350
                              },
                              primaryCPICH_TX_Power: OMIT,
                              readSFN_Indicator: GcTRUE,
                              tx_DiversityIndicator: GcFALSE
                            }
                          ],
                          cellSelectionReselectionInfo: OMIT
                        }
                      }
                    ]
                  },
                  intraFreqMeasQuantity:
                  {
                    filterCoefficient: OMIT,
                    modeSpecificInfo:
                    [
                      fdd:
                      {
                        intraFreqMeasQuantity_FDD: cpich_RSCP
                      }
                    ]
                  },
                  intraFreqReportingQuantityForRACH: OMIT,
                  maxReportedCellsOnRACH: OMIT,
                  reportingInfoForCellDCH:
                  {
                    intraFreqReportingQuantity:
                    {
                      activeSetReportingQuantities:
                      {
                        dummy: noReport,
                        cellIdentity_reportingIndicator: GcTRUE,
                        cellSynchronisationInfoReportingIndicator: GcFALSE,
                        modeSpecificInfo:
                        [
                          fdd:
                          {
                            cpich_Ec_N0_reportingIndicator: GcFALSE,
                            cpich_RSCP_reportingIndicator: GcTRUE,
                            pathloss_reportingIndicator: GcFALSE
                          }
                        ]
                      },
                      monitoredSetReportingQuantities:
                      {
                        dummy: noReport,
                        cellIdentity_reportingIndicator: GcTRUE,
                        cellSynchronisationInfoReportingIndicator: GcTRUE,
                        modeSpecificInfo:
                        [
                          fdd:
                          {
                            cpich_Ec_N0_reportingIndicator: GcFALSE,
                            cpich_RSCP_reportingIndicator: GcTRUE,
                            pathloss_reportingIndicator: GcFALSE
                          }
                        ]
                      },
                      detectedSetReportingQuantities: OMIT
                    },
                    measurementReportingMode:
                    {
                      measurementReportTransferMode: acknowledgedModeRLC,
                      periodicalOrEventTrigger: eventTrigger
                    },
                    reportCriteria:
                    [
                      intraFreqReportingCriteria:
                      {
                        eventCriteriaList:
                        [
                          {
                            event:
                            [
                              e1a:
                              {
                                triggeringCondition: monitoredSetCellsOnly,
                                reportingRange: 5,
                                forbiddenAffectCellList: OMIT,
                                w: 1,
                                reportDeactivationThreshold: t2,
                                reportingAmount: ra4,
                                reportingInterval: ri4
                              }
                            ],
                            hysteresis: 0,
                            timeToTrigger: ttt640,
                            reportingCellStatus:
                            [
                              withinActiveAndOrMonitoredUsedFreq: e3
                            ]
                          },

                          {
                            event:
                            [
                              e1b:
                              {
                                triggeringCondition: activeSetCellsOnly,
                                reportingRange: 5,
                                forbiddenAffectCellList: OMIT,
                                w: 1
                              }
                            ],
                            hysteresis: 0,
                            timeToTrigger: ttt640,
                            reportingCellStatus:
                            [
                              withinActiveAndOrMonitoredUsedFreq: e3
                            ]
                          },

                          {
                            event:
                            [
                              e1c:
                              {
                                replacementActivationThreshold: t3,
                                reportingAmount: ra4,
                                reportingInterval: ri4
                              }
                            ],
                            hysteresis: 0,
                            timeToTrigger: ttt640,
                            reportingCellStatus:
                            [
                              withinActiveAndOrMonitoredUsedFreq: e3
                            ]
                          }
                        ]
                      }
                    ]
                  }
                },
                interFreqMeasurementSysInfo:
                {
                  interFreqCellInfoSI_List:
                  {
                    removedInterFreqCellList: OMIT,
                    newInterFreqCellList:
                    [
                      {
                        interFreqCellID: 0,
                        frequencyInfo:
                        {
                          modeSpecificInfo:
                          [
                            fdd:
                            {
                              uarfcn_UL: OMIT,
                              uarfcn_DL: 10700
                            }
                          ]
                        },
                        cellInfo:
                        {
                          cellIndividualOffset: OMIT,
                          referenceTimeDifferenceToCell: OMIT,
                          modeSpecificInfo:
                          [
                            fdd:
                            {
                              primaryCPICH_Info:
                              {
                                primaryScramblingCode: 100
                              },
                              primaryCPICH_TX_Power: OMIT,
                              readSFN_Indicator: GcFALSE,
                              tx_DiversityIndicator: GcFALSE
                            }
                          ],
                          cellSelectionReselectionInfo: OMIT
                        }
                      },

                      {
                        interFreqCellID: 1,
                        frequencyInfo: OMIT,
                        cellInfo:
                        {
                          cellIndividualOffset: OMIT,
                          referenceTimeDifferenceToCell: OMIT,
                          modeSpecificInfo:
                          [
                            fdd:
                            {
                              primaryCPICH_Info:
                              {
                                primaryScramblingCode: 150
                              },
                              primaryCPICH_TX_Power: OMIT,
                              readSFN_Indicator: GcFALSE,
                              tx_DiversityIndicator: GcFALSE
                            }
                          ],
                          cellSelectionReselectionInfo: OMIT
                        }
                      },

                      {
                        interFreqCellID: 2,
                        frequencyInfo: OMIT,
                        cellInfo:
                        {
                          cellIndividualOffset: OMIT,
                          referenceTimeDifferenceToCell: OMIT,
                          modeSpecificInfo:
                          [
                            fdd:
                            {
                              primaryCPICH_Info:
                              {
                                primaryScramblingCode: 200
                              },
                              primaryCPICH_TX_Power: OMIT,
                              readSFN_Indicator: GcFALSE,
                              tx_DiversityIndicator: GcFALSE
                            }
                          ],
                          cellSelectionReselectionInfo: OMIT
                        }
                      },

                      {
                        interFreqCellID: 6,
                        frequencyInfo: OMIT,
                        cellInfo:
                        {
                          cellIndividualOffset: OMIT,
                          referenceTimeDifferenceToCell: OMIT,
                          modeSpecificInfo:
                          [
                            fdd:
                            {
                              primaryCPICH_Info:
                              {
                                primaryScramblingCode: 400
                              },
                              primaryCPICH_TX_Power: OMIT,
                              readSFN_Indicator: GcFALSE,
                              tx_DiversityIndicator: GcFALSE
                            }
                          ],
                          cellSelectionReselectionInfo: OMIT
                        }
                      },

                      {
                        interFreqCellID: 7,
                        frequencyInfo: OMIT,
                        cellInfo:
                        {
                          cellIndividualOffset: OMIT,
                          referenceTimeDifferenceToCell: OMIT,
                          modeSpecificInfo:
                          [
                            fdd:
                            {
                              primaryCPICH_Info:
                              {
                                primaryScramblingCode: 450
                              },
                              primaryCPICH_TX_Power: OMIT,
                              readSFN_Indicator: GcFALSE,
                              tx_DiversityIndicator: GcFALSE
                            }
                          ],
                          cellSelectionReselectionInfo: OMIT
                        }
                      }
                    ]
                  }
                }
              }
            ],
            interRATMeasurementSysInfo: OMIT
          }
        ],
        trafficVolumeMeasSysInfo: OMIT,
        dummy: OMIT
      },
      nonCriticalExtensions: OMIT
    }

TTCN Assignment: tcv_SIB12 :=

(To search, click here and then press Ctrl+F)

    {
      fach_MeasurementOccasionInfo: OMIT,
      measurementControlSysInfo:
      {
        use_of_HCS:
        [
          hcs_not_used:
          {
            cellSelectQualityMeasure:
            [
              cpich_RSCP:
              {
                intraFreqMeasurementSysInfo: OMIT,
                interFreqMeasurementSysInfo: OMIT
              }
            ],
            interRATMeasurementSysInfo: OMIT
          }
        ],
        trafficVolumeMeasSysInfo: OMIT,
        dummy: OMIT
      },
      nonCriticalExtensions: OMIT
    }

TTCN Assignment: tcv_SIB1 :=

(To search, click here and then press Ctrl+F)

    {
      cn_CommonGSM_MAP_NAS_SysInfo: '0001'O,
      cn_DomainSysInfoList:
      [
        {
          cn_DomainIdentity: ps_domain,
          cn_Type:
          [
            gsm_MAP: '0501'O
          ],
          cn_DRX_CycleLengthCoeff: 7
        },

        {
          cn_DomainIdentity: cs_domain,
          cn_Type:
          [
            gsm_MAP: '0000'O
          ],
          cn_DRX_CycleLengthCoeff: 7
        }
      ],
      ue_ConnTimersAndConstants:
      {
        t_301: OMIT,
        n_301: OMIT,
        t_302: OMIT,
        n_302: OMIT,
        t_304: OMIT,
        n_304: OMIT,
        t_305: OMIT,
        t_307: OMIT,
        t_308: OMIT,
        t_309: OMIT,
        t_310: OMIT,
        n_310: OMIT,
        t_311: OMIT,
        t_312: OMIT,
        n_312: OMIT,
        t_313: OMIT,
        n_313: OMIT,
        t_314: OMIT,
        t_315: OMIT,
        n_315: OMIT,
        t_316: OMIT,
        t_317: OMIT
      },
      ue_IdleTimersAndConstants:
      {
        t_300: ms4000,
        n_300: 3,
        t_312: 10,
        n_312: s1
      },
      v3a0NonCriticalExtensions: OMIT
    }

TTCN Assignment: seg1 :=

(To search, click here and then press Ctrl+F)

    '1100010000000000000001011000100000101000000010100001000000000000000001000000000000000000000011000111010000'B

TTCN Assignment: seg2 :=

(To search, click here and then press Ctrl+F)

    '1100010000000000000001011000100000101000000010100001000000000000000001000000000000000000000011000111010000'B

TTCN Assignment: tcv_SIB3 :=

(To search, click here and then press Ctrl+F)

    {
      sib4indicator: GcTRUE,
      cellIdentity: '0000000000000000000000000011'B,
      cellSelectReselectInfo:
      {
        mappingInfo: OMIT,
        cellSelectQualityMeasure:
        [
          cpich_RSCP: NULL
        ],
        modeSpecificInfo:
        [
          fdd:
          {
            s_Intrasearch: 8,
            s_Intersearch: 8,
            s_SearchHCS: OMIT,
            rat_List:
            [
              {
                rat_Identifier: gsm,
                s_SearchRAT: -16,
                s_HCS_RAT: OMIT,
                s_Limit_SearchRAT: 0
              }
            ],
            q_QualMin: -24,
            q_RxlevMin: -40
          }
        ],
        q_Hyst_l_S: 2,
        t_Reselection_S: 0,
        hcs_ServingCellInformation: OMIT,
        maxAllowedUL_TX_Power: 21
      },
      cellAccessRestriction:
      {
        cellBarred:
        [
          notBarred: NULL
        ],
        cellReservedForOperatorUse: notReserved,
        cellReservationExtension: notReserved,
        accessClassBarredList:
        [
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred
        ]
      },
      nonCriticalExtensions: OMIT
    }

TTCN Assignment: seg1 :=

(To search, click here and then press Ctrl+F)

    '0100000000000000000000000000110010110111000110000000000000010000000000100100001000000100011111111111111111111111'B

TTCN Assignment: tcv_SIB4 :=

(To search, click here and then press Ctrl+F)

    {
      cellIdentity: '0000000000000000000000000011'B,
      cellSelectReselectInfo:
      {
        mappingInfo: OMIT,
        cellSelectQualityMeasure:
        [
          cpich_RSCP: NULL
        ],
        modeSpecificInfo:
        [
          fdd:
          {
            s_Intrasearch: 8,
            s_Intersearch: 8,
            s_SearchHCS: OMIT,
            rat_List:
            [
              {
                rat_Identifier: gsm,
                s_SearchRAT: -16,
                s_HCS_RAT: OMIT,
                s_Limit_SearchRAT: 0
              }
            ],
            q_QualMin: -24,
            q_RxlevMin: -40
          }
        ],
        q_Hyst_l_S: 0,
        t_Reselection_S: 0,
        hcs_ServingCellInformation: OMIT,
        maxAllowedUL_TX_Power: 21
      },
      cellAccessRestriction:
      {
        cellBarred:
        [
          notBarred: NULL
        ],
        cellReservedForOperatorUse: notReserved,
        cellReservationExtension: notReserved,
        accessClassBarredList: OMIT
      },
      nonCriticalExtensions: OMIT
    }

TTCN Assignment: seg1 :=

(To search, click here and then press Ctrl+F)

    '00000000000000000000000000011001011011100011000000000000001000000000010010000000000010001110111'B

TTCN Assignment: tcv_Segs :=

(To search, click here and then press Ctrl+F)

    {
      segCount: 3,
      seg1: '000101010100010000111110000000001111111101000011111111111111110111010010000100001111000000101001000011000000101010100101010110000000000000001100110001011011010101111110001010111010000011111110100000111111101000001111111010'B,
      seg2: '000011111111010000000000000000001101011000110100010000111111010011100101000001100001000011001010000000110000001110000001000000010110000010000000111000000000100010000110010000101001100100001010000000000011000000010001000101'B,
      seg3: '1100101011010110100000000000011110001000011000000001011011011011011000100000000001000011000010001001010000001011011010000000010000'B,
      seg4: OMIT,
      seg5: OMIT,
      seg6: OMIT,
      seg7: OMIT,
      seg8: OMIT,
      seg9: OMIT,
      seg10: OMIT,
      seg11: OMIT,
      seg12: OMIT,
      seg13: OMIT,
      seg14: OMIT,
      seg15: OMIT,
      seg16: OMIT
    }

TTCN Assignment: scheduling :=

(To search, click here and then press Ctrl+F)

    {
      scheduling:
      {
        segCount: 3,
        sib_Pos:
        [
          rep64: 19
        ],
        sib_PosOffsetInfo:
        [
          so4,
          so2
        ]
      }
    }

TTCN Assignment: tcv_Segs :=

(To search, click here and then press Ctrl+F)

    {
      segCount: 1,
      seg1: '0000001010010001'B,
      seg2: OMIT,
      seg3: OMIT,
      seg4: OMIT,
      seg5: OMIT,
      seg6: OMIT,
      seg7: OMIT,
      seg8: OMIT,
      seg9: OMIT,
      seg10: OMIT,
      seg11: OMIT,
      seg12: OMIT,
      seg13: OMIT,
      seg14: OMIT,
      seg15: OMIT,
      seg16: OMIT
    }

TTCN Assignment: tcv_Segs :=

(To search, click here and then press Ctrl+F)

    {
      segCount: 1,
      seg1: '100000101000000010000001'B,
      seg2: OMIT,
      seg3: OMIT,
      seg4: OMIT,
      seg5: OMIT,
      seg6: OMIT,
      seg7: OMIT,
      seg8: OMIT,
      seg9: OMIT,
      seg10: OMIT,
      seg11: OMIT,
      seg12: OMIT,
      seg13: OMIT,
      seg14: OMIT,
      seg15: OMIT,
      seg16: OMIT
    }

TTCN Assignment: tcv_SIB7 :=

(To search, click here and then press Ctrl+F)

    {
      modeSpecificInfo:
      [
        fdd:
        {
          ul_Interference: -100
        }
      ],
      prach_Information_SIB5_List:
      [
        2
      ],
      prach_Information_SIB6_List:
      [
        2
      ],
      expirationTimeFactor: OMIT,
      nonCriticalExtensions: OMIT
    }

TTCN Assignment: seg2 :=

(To search, click here and then press Ctrl+F)

    '0100000000000000000000000000110010110111000110000000000000010000000000100100001000000100011111111111111111111111'B

TTCN Assignment: seg2 :=

(To search, click here and then press Ctrl+F)

    '00000000000000000000000000011001011011100011000000000000001000000000010010000000000010001110111'B

TTCN Assignment: tcv_Segs :=

(To search, click here and then press Ctrl+F)

    {
      segCount: 2,
      seg1: '001000001101100100001010001100001001111101000100100000010100101100101001010000101010111101000010001000100011001001010101000000010010100001010010101000011000010010100010000010100001000011000010010100100110101010000110000100'B,
      seg2: '10101001001100000001010011100110000001000110010000100000100001001001011000100001000001001100100000100011000001011001000000100011100001011100001000'B,
      seg3: OMIT,
      seg4: OMIT,
      seg5: OMIT,
      seg6: OMIT,
      seg7: OMIT,
      seg8: OMIT,
      seg9: OMIT,
      seg10: OMIT,
      seg11: OMIT,
      seg12: OMIT,
      seg13: OMIT,
      seg14: OMIT,
      seg15: OMIT,
      seg16: OMIT
    }

TTCN Assignment: scheduling :=

(To search, click here and then press Ctrl+F)

    {
      scheduling:
      {
        segCount: 2,
        sib_Pos:
        [
          rep64: 29
        ],
        sib_PosOffsetInfo:
        [
          so2
        ]
      }
    }

TTCN Assignment: tcv_Segs :=

(To search, click here and then press Ctrl+F)

    {
      segCount: 1,
      seg1: '000000000'B,
      seg2: OMIT,
      seg3: OMIT,
      seg4: OMIT,
      seg5: OMIT,
      seg6: OMIT,
      seg7: OMIT,
      seg8: OMIT,
      seg9: OMIT,
      seg10: OMIT,
      seg11: OMIT,
      seg12: OMIT,
      seg13: OMIT,
      seg14: OMIT,
      seg15: OMIT,
      seg16: OMIT
    }

TTCN Assignment: tcv_SIB18 :=

(To search, click here and then press Ctrl+F)

    {
      idleModePLMNIdentities:
      {
        plmnsOfIntraFreqCellsList: OMIT,
        plmnsOfInterFreqCellsList:
        [
          {
            plmn_Identity:
            {
              mcc:
              [
                0,
                0,
                1
              ],
              mnc:
              [
                0,
                1
              ]
            }
          }
        ],
        plmnsOfInterRATCellsList: OMIT
      },
      connectedModePLMNIdentities: OMIT,
      nonCriticalExtensions: OMIT
    }

TTCN Assignment: tcv_Segs :=

(To search, click here and then press Ctrl+F)

    {
      segCount: 1,
      seg1: '00010000101110001000001100110000010010010101111000101001110100000000010111100010001101110011100010010010'B,
      seg2: OMIT,
      seg3: OMIT,
      seg4: OMIT,
      seg5: OMIT,
      seg6: OMIT,
      seg7: OMIT,
      seg8: OMIT,
      seg9: OMIT,
      seg10: OMIT,
      seg11: OMIT,
      seg12: OMIT,
      seg13: OMIT,
      seg14: OMIT,
      seg15: OMIT,
      seg16: OMIT
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10837
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 250,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 321,
      sfnOffset: 3000,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '002'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000010'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NoDPCH,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 3000,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_Segs :=

(To search, click here and then press Ctrl+F)

    {
      segCount: 1,
      seg1: '0011000000000000100000000010010110101110000100010000000000100000100010110000111000100010110001011000100010100001111000100110100010011110010010010011000100010000'B,
      seg2: OMIT,
      seg3: OMIT,
      seg4: OMIT,
      seg5: OMIT,
      seg6: OMIT,
      seg7: OMIT,
      seg8: OMIT,
      seg9: OMIT,
      seg10: OMIT,
      seg11: OMIT,
      seg12: OMIT,
      seg13: OMIT,
      seg14: OMIT,
      seg15: OMIT,
      seg16: OMIT
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10837
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 250,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 321,
      sfnOffset: 3000,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '002'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000010'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NoDPCH,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 3000,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 30,
      priScrmCode: 150,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '02'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB_NoConn,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 1000,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10837
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 250,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 321,
      sfnOffset: 3000,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '002'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000010'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NoDPCH,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 3000,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_CellInfoD :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10837
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 250,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 321,
      sfnOffset: 3000,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '002'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000010'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB_NoConn,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 3000,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10837
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 250,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 321,
      sfnOffset: 3000,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '002'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000010'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB_NoConn,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 3000,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10837
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 250,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 321,
      sfnOffset: 3000,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '002'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000010'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB_NoConn,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 3000,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_CellInfoD :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10837
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 250,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 321,
      sfnOffset: 3000,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '002'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000010'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 3000,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10837
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 250,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 321,
      sfnOffset: 3000,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '002'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000010'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 3000,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_StartList :=

(To search, click here and then press Ctrl+F)

    [
      {
        cn_DomainIdentity: ps_domain,
        start_Value: '00000000000000000010'B
      },

      {
        cn_DomainIdentity: cs_domain,
        start_Value: '00000000000000000010'B
      }
    ]

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10837
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 250,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 321,
      sfnOffset: 3000,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '002'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000010'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 3000,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_AuthXDOUT :=

(To search, click here and then press Ctrl+F)

    '01010101010001000111011101100110000100010000000000110011001000101101110111001100111111111110111010011001100010001011101110101010'B

TTCN Assignment: tcv_AuthAUTN_2 :=

(To search, click here and then press Ctrl+F)

    '00000000000000000101010101000100011101110110011000010001000000000011001100100010'B

TTCN Assignment: tcv_AuthAUTN :=

(To search, click here and then press Ctrl+F)

    '01100110000100010000000000110011001000101101110100000000000000000101010101000100011101110110011000010001000000000011001100100010'B

TTCN Assignment: tcv_AuthIK :=

(To search, click here and then press Ctrl+F)

    '01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100'B

TTCN Assignment: tcv_AuthCK :=

(To search, click here and then press Ctrl+F)

    '01000100011101110110011000010001000000000011001100100010110111011100110011111111111011101001100110001000101110111010101001010101'B

TTCN Assignment: tcv_AuthXRES :=

(To search, click here and then press Ctrl+F)

    '01010101010001000111011101100110000100010000000000110011001000101101110111001100111111111110111010011001100010001011101110101010'B

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10837
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 250,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 321,
      sfnOffset: 3000,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '002'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000010'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 3000,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: dL_Integrity :=

(To search, click here and then press Ctrl+F)

    {
      integrityProtectionModeCommand:
      [
        startIntegrityProtection:
        {
          integrityProtInitNumber: '00001111000011110000111100001111'B
        }
      ],
      integrityProtectionAlgorithm: uia1
    }

TTCN Assignment: dl_IntegrityCheckInfo :=

(To search, click here and then press Ctrl+F)

    {
      messageAuthenticationCode: '00000000000000000000000000000000'B,
      rrc_MessageSequenceNumber: 0
    }

TTCN Assignment: tcv_CellInfoD :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10837
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 250,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 321,
      sfnOffset: 3000,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '002'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000010'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 3000,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10837
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 250,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 321,
      sfnOffset: 3000,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '002'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000010'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 3000,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_AuthXDOUT :=

(To search, click here and then press Ctrl+F)

    '01010101010001000111011101100110000100010000000000110011001000101101110111001100111111111110111010011001100010001011101110101010'B

TTCN Assignment: tcv_AuthAUTN_2 :=

(To search, click here and then press Ctrl+F)

    '00000000000000000101010101000100011101110110011000010001000000000011001100100010'B

TTCN Assignment: tcv_AuthAUTN :=

(To search, click here and then press Ctrl+F)

    '01100110000100010000000000110011001000101101110100000000000000000101010101000100011101110110011000010001000000000011001100100010'B

TTCN Assignment: tcv_PS_AuthIK :=

(To search, click here and then press Ctrl+F)

    '01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100'B

TTCN Assignment: tcv_PS_AuthCK :=

(To search, click here and then press Ctrl+F)

    '01000100011101110110011000010001000000000011001100100010110111011100110011111111111011101001100110001000101110111010101001010101'B

TTCN Assignment: tcv_AuthXRES :=

(To search, click here and then press Ctrl+F)

    '01010101010001000111011101100110000100010000000000110011001000101101110111001100111111111110111010011001100010001011101110101010'B

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10837
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 250,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 321,
      sfnOffset: 3000,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '002'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000010'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 3000,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: dL_Integrity :=

(To search, click here and then press Ctrl+F)

    {
      integrityProtectionModeCommand:
      [
        modify:
        {
          dl_IntegrityProtActivationInfo:
          {
            rrc_MessageSequenceNumberList:
            [
              0,
              0,
              1,
              2,
              0
            ]
          }
        }
      ],
      integrityProtectionAlgorithm: uia1
    }

TTCN Assignment: tcv_CellInfoD :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10837
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 250,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 321,
      sfnOffset: 3000,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '002'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000010'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 3000,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10837
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 250,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 321,
      sfnOffset: 3000,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '002'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000010'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 3000,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10837
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 250,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 321,
      sfnOffset: 3000,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '002'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000010'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 3000,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10837
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 250,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 321,
      sfnOffset: 3000,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '002'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000010'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 3000,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_CellInfoD :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10837
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 250,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 321,
      sfnOffset: 3000,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '002'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000010'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB_NoConn,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 3000,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_CellIndInfo :=

(To search, click here and then press Ctrl+F)

    {
      cs_cipheringStarted: GcFALSE,
      ps_cipheringStarted: GcFALSE,
      recentSecureDomain: cs_domain,
      dL_CipherMode:
      [
        dummy: NULL
      ],
      uL_CipherMode: OMIT,
      cipheringAlgorithmCapability: '0000000000000011'B,
      integrityStarted: GcFALSE,
      dL_Integrity:
      {
        integrityProtectionModeCommand:
        [
          startIntegrityProtection:
          {
            integrityProtInitNumber: '00001111000011110000111100001111'B
          }
        ],
        integrityProtectionAlgorithm: uia1
      },
      uL_Integrity: OMIT,
      dl_IntegrityCheckInfo: OMIT,
      start_CS: '00000000000000000000'B,
      start_PS: '00000000000000000000'B
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10837
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 250,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 321,
      sfnOffset: 3000,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '002'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000010'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB_NoConn,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 3000,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10837
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 250,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 321,
      sfnOffset: 3000,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '002'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000010'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB_NoConn,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 3000,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10837
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 250,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 321,
      sfnOffset: 3000,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '002'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000010'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB_NoConn,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 3000,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_InitialUE_Id :=

(To search, click here and then press Ctrl+F)

    [
      tmsi_and_LAI:
      {
        tmsi: '00010001001000100011001101000100'B,
        lai:
        {
          plmn_Identity:
          {
            mcc:
            [
              0,
              0,
              2
            ],
            mnc:
            [
              0,
              1
            ]
          },
          lac: '0000000000000001'B
        }
      }
    ]

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10837
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 250,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 321,
      sfnOffset: 3000,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '002'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000010'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB_NoConn,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 3000,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_CellInfoD :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10837
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 250,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 321,
      sfnOffset: 3000,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '002'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000010'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 3000,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10837
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 250,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 321,
      sfnOffset: 3000,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '002'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000010'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 3000,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_StartList :=

(To search, click here and then press Ctrl+F)

    [
      {
        cn_DomainIdentity: ps_domain,
        start_Value: '00000000000000000010'B
      },

      {
        cn_DomainIdentity: cs_domain,
        start_Value: '00000000000000000010'B
      }
    ]

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10837
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 250,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 321,
      sfnOffset: 3000,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '002'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000010'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 3000,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10837
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 250,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 321,
      sfnOffset: 3000,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '002'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000010'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 3000,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_CellInfoD :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10837
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 250,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 321,
      sfnOffset: 3000,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '002'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000010'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB_NoConn,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 3000,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_CellIndInfo :=

(To search, click here and then press Ctrl+F)

    {
      cs_cipheringStarted: GcFALSE,
      ps_cipheringStarted: GcFALSE,
      recentSecureDomain: cs_domain,
      dL_CipherMode:
      [
        dummy: NULL
      ],
      uL_CipherMode: OMIT,
      cipheringAlgorithmCapability: '0000000000000011'B,
      integrityStarted: GcFALSE,
      dL_Integrity:
      {
        integrityProtectionModeCommand:
        [
          startIntegrityProtection:
          {
            integrityProtInitNumber: '00001111000011110000111100001111'B
          }
        ],
        integrityProtectionAlgorithm: uia1
      },
      uL_Integrity: OMIT,
      dl_IntegrityCheckInfo: OMIT,
      start_CS: '00000000000000000000'B,
      start_PS: '00000000000000000000'B
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 10,
      priScrmCode: 100,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NotConfigured,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 0,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 30,
      priScrmCode: 150,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '02'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NoDPCH,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 1000,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 30,
      priScrmCode: 150,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '02'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NoDPCH,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 1000,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 30,
      priScrmCode: 150,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '02'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NoDPCH,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 1000,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 30,
      priScrmCode: 150,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '02'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NoDPCH,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 1000,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_CellInfoB :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 30,
      priScrmCode: 150,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '02'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000001'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NotConfigured,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 1000,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 2,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 200,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 1,
      nmo: '00'O,
      ura_Identity: '0000000000000010'B,
      t3212: '1E'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NotConfigured,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 2000,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10837
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 250,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 321,
      sfnOffset: 3000,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '002'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000010'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB_NoConn,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 3000,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10837
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 250,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 321,
      sfnOffset: 3000,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '002'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000010'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB_NoConn,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 3000,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10837
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 250,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 321,
      sfnOffset: 3000,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '002'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000010'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB_NoConn,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 3000,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10837
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 250,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 321,
      sfnOffset: 3000,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '002'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000010'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB_NoConn,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 3000,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10837
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 250,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 321,
      sfnOffset: 3000,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '002'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000010'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB_NoConn,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 3000,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_CellInfoD :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10837
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 250,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 321,
      sfnOffset: 3000,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '002'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 0,
      nmo: '01'O,
      ura_Identity: '0000000000000010'B,
      t3212: '00'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NotConfigured,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 3000,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 4,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10837
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 300,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 833,
      sfnOffset: 3000,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 1,
      nmo: '00'O,
      ura_Identity: '0000000000000011'B,
      t3212: '1E'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NotConfigured,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 4000,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 5,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10837
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 350,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 6577,
      sfnOffset: 678,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 1,
      nmo: '00'O,
      ura_Identity: '0000000000000011'B,
      t3212: '1E'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NotConfigured,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 5000,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 6,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 400,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 7253,
      sfnOffset: 1356,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 1,
      nmo: '00'O,
      ura_Identity: '0000000000000100'B,
      t3212: '1E'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NotConfigured,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 6000,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }

TTCN Assignment: tcv_TmpCellInfo :=

(To search, click here and then press Ctrl+F)

    {
      cellId: 7,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 450,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 4351,
      sfnOffset: 2034,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 1,
      nmo: '00'O,
      ura_Identity: '0000000000000100'B,
      t3212: '1E'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NotConfigured,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 7000,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }