|  |  | NAS_wk34-GMM-Routing_Area_updating-PS_only_RAU-tc_12_4_1_2 | Contains 10301 lines/items
| StartTimer:[1] t_Guard [300] 300 s Attach:[2] Enter Test Step ts_InitVariables( )
| Attach:[1] Enter Test Step ts_InitVariables::lt_CalculateFrequencyInfo( )
| Attach:[10] Enter Test Step ts_InitVariables::lt_CalculateFreqMid( )
| Attach:[13] Enter Test Step ts_InitVariables::lt_CheckFreqSeperation( 10700 )
| Assignment:[30] tcv_Res := GcTRUE Attach:[13] Exit Test Step ts_InitVariables::lt_CheckFreqSeperation
Assignment:[17] tcv_FreqInfoMid := { modeSpecificInfo: [fdd: { uarfcn_UL: OMIT, uarfcn_DL: 10700 } ]} Attach:[10] Exit Test Step ts_InitVariables::lt_CalculateFreqMid
Attach:[11] Enter Test Step ts_InitVariables::lt_CalculateFreqHigh( )
| Attach:[18] Enter Test Step ts_InitVariables::lt_CheckFreqSeperation( 10837 )
| Assignment:[30] tcv_Res := GcTRUE Attach:[18] Exit Test Step ts_InitVariables::lt_CheckFreqSeperation
Assignment:[22] tcv_FreqInfoHigh := { modeSpecificInfo: [fdd: { uarfcn_UL: OMIT, uarfcn_DL: 10837 } ]} Attach:[11] Exit Test Step ts_InitVariables::lt_CalculateFreqHigh
Attach:[12] Enter Test Step ts_InitVariables::lt_CalculateFreqLow( )
| Attach:[23] Enter Test Step ts_InitVariables::lt_CheckFreqSeperation( 10563 )
| Assignment:[30] tcv_Res := GcTRUE Attach:[23] Exit Test Step ts_InitVariables::lt_CheckFreqSeperation
Assignment:[27] tcv_FreqInfoLow := { modeSpecificInfo: [fdd: { uarfcn_UL: OMIT, uarfcn_DL: 10563 } ]} Attach:[12] Exit Test Step ts_InitVariables::lt_CalculateFreqLow
Attach:[1] Exit Test Step ts_InitVariables::lt_CalculateFrequencyInfo
Attach:[2] Enter Test Step ts_InitVariables::lt_Init_SSInfo_CellA( )
| Assignment:[48] tcv_CellInfoA := (view Assignment) Attach:[2] Exit Test Step ts_InitVariables::lt_Init_SSInfo_CellA
Attach:[3] Enter Test Step ts_InitVariables::lt_Init_SSInfo_CellB( )
| Assignment:[49] tcv_CellInfoB := (view Assignment) Attach:[3] Exit Test Step ts_InitVariables::lt_Init_SSInfo_CellB
Attach:[4] Enter Test Step ts_InitVariables::lt_Init_SSInfo_CellC( )
| Assignment:[50] tcv_CellInfoC := (view Assignment) Attach:[4] Exit Test Step ts_InitVariables::lt_Init_SSInfo_CellC
Attach:[5] Enter Test Step ts_InitVariables::lt_Init_SSInfo_CellD( )
| Assignment:[51] tcv_CellInfoD := (view Assignment) Attach:[5] Exit Test Step ts_InitVariables::lt_Init_SSInfo_CellD
Attach:[6] Enter Test Step ts_InitVariables::lt_Init_SSInfo_CellE( )
| Assignment:[52] tcv_CellInfoE := (view Assignment) Attach:[6] Exit Test Step ts_InitVariables::lt_Init_SSInfo_CellE
Attach:[7] Enter Test Step ts_InitVariables::lt_Init_SSInfo_CellF( )
| Assignment:[53] tcv_CellInfoF := (view Assignment) Attach:[7] Exit Test Step ts_InitVariables::lt_Init_SSInfo_CellF
Attach:[8] Enter Test Step ts_InitVariables::lt_Init_SSInfo_CellG( )
| Assignment:[54] tcv_CellInfoG := (view Assignment) Attach:[8] Exit Test Step ts_InitVariables::lt_Init_SSInfo_CellG
Attach:[9] Enter Test Step ts_InitVariables::lt_Init_SSInfo_CellH( )
| Assignment:[55] tcv_CellInfoH := (view Assignment) Attach:[9] Exit Test Step ts_InitVariables::lt_Init_SSInfo_CellH
Attach:[2] Exit Test Step ts_InitVariables
Assignment:[3] tcv_NumOfPLMN := 2 Assignment:[3] nmo := '01'O Assignment:[3] attenuationLevel := 30 Assignment:[3] nmo := '01'O Assignment:[3] rac := '02'O Assignment:[3] attFlag := 0 Assignment:[3] t3212 := '00'O Assignment:[3] nmo := '01'O Assignment:[3] mcc := '002'H Assignment:[3] attFlag := 0 Assignment:[3] t3212 := '00'O Attach:[4] Enter Test Step ts_GMM_SetOpModeC_OrA( )
| Attach:[4] Enter Test Step ts_MMI_SetOpModeA( )
| 00:00:05.590 - Primitive: MMI_CmdReq Send event:[1] Ut ! MMI_CmdReq = PDU (view PDU) 00:00:06.950 - Primitive: MMI_CmdCnf begin "ca_MMI_CmdCnf" of type MMI_CmdCnf (SEQUENCE) [UNIVERSAL 16] begin "result" of type BOOLEAN [UNIVERSAL 1] matching GcTRUE against GcTRUE end "result" of type BOOLEAN end "ca_MMI_CmdCnf" of type MMI_CmdCnf Receive event:[2] Ut ? MMI_CmdCnf = PDU: { result: GcTRUE , resultString: OMIT} Assignment:[3] tcv_UE_OpMode := opModeA Attach:[4] Exit Test Step ts_MMI_SetOpModeA
Attach:[4] Exit Test Step ts_GMM_SetOpModeC_OrA
Attach:[5] Enter Test Step ts_GMM_Config_CellA_CellB( )
| Attach:[1] Enter Test Step ts_SS_CreateCellDCH( 0 )
| Attach:[1] Enter Test Step ts_SS_CellCfg( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[4] Enter Test Step ts_SS_CellCfg::lt_CelllsAlreadyStarted( 0 )
| Attach:[11] Enter Test Step ts_CountConfiguredCell( )
| Assignment:[1] tcv_NumCfgCell := 0 Attach:[2] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 0 , frequenc ...
| (view Test Step parameters) Attach:[2] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[3] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 1 , frequenc ...
| (view Test Step parameters) Attach:[3] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[4] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 2 , frequenc ...
| (view Test Step parameters) Attach:[4] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[5] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 3 , frequenc ...
| (view Test Step parameters) Attach:[5] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[6] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 4 , frequenc ...
| (view Test Step parameters) Attach:[6] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[7] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 5 , frequenc ...
| (view Test Step parameters) Attach:[7] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[8] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 6 , frequenc ...
| (view Test Step parameters) Attach:[8] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[9] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 7 , frequenc ...
| (view Test Step parameters) Attach:[9] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[11] Exit Test Step ts_CountConfiguredCell
Attach:[13] Enter Test Step ts_MM_PwrOrUSIM_Off( GcTRUE )
| Attach:[4] Enter Test Step ts_MMI_UE_SwitchOff( )
| 00:00:06.950 - Primitive: MMI_CmdReq Send event:[2] Ut ! MMI_CmdReq = PDU: { cmd: "Please switch off the UE" } 00:00:07.540 - Primitive: MMI_CmdCnf begin "ca_MMI_CmdCnf" of type MMI_CmdCnf (SEQUENCE) [UNIVERSAL 16] begin "result" of type BOOLEAN [UNIVERSAL 1] matching GcTRUE against GcTRUE end "result" of type BOOLEAN end "ca_MMI_CmdCnf" of type MMI_CmdCnf Receive event:[3] Ut ? MMI_CmdCnf = PDU: { result: GcTRUE , resultString: OMIT} Assignment:[4] tcv_UE_SwitchedOn := GcFALSE Attach:[4] Exit Test Step ts_MMI_UE_SwitchOff
Attach:[13] Exit Test Step ts_MM_PwrOrUSIM_Off
00:00:07.540 - Primitive: CPHY_Ini_REQ Send event:[15] CPHY ! CPHY_Ini_REQ = PDU: defaultRadioEnvironment 00:00:07.960 - Primitive: CPHY_Ini_CNF begin "car_IniCnf" of type CPHY_Ini_CNF (SEQUENCE) [UNIVERSAL 16] begin "confirmation" of type NULL [UNIVERSAL 5] matching NULL against NULL end "confirmation" of type NULL end "car_IniCnf" of type CPHY_Ini_CNF Receive event:[16] CPHY ? CPHY_Ini_CNF = PDU: { confirmation: NULL} Assignment:[17] tCell := 0 Attach:[4] Exit Test Step ts_SS_CellCfg::lt_CelllsAlreadyStarted
00:00:07.960 - Primitive: CPHY_Cell_Config_REQ Send event:[6] CPHY ! CPHY_Cell_Config_REQ = PDU (view PDU) 00:00:07.980 - Primitive: CPHY_Cell_Config_CNF begin "ca_CellCfgCnf" of type CPHY_Cell_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER end "ca_CellCfgCnf" of type CPHY_Cell_Config_CNF Receive event:[7] CPHY ? CPHY_Cell_Config_CNF = PDU: { cellId: 0 } Attach:[8] Enter Test Step ts_SaveCellInfo( 0 )
| Assignment:[2] tcv_CellInfoA := (view Assignment) Attach:[8] Exit Test Step ts_SaveCellInfo
Attach:[1] Exit Test Step ts_SS_CellCfg
Attach:[2] Enter Test Step ts_SS_BCH_SCH_CPICH_Cfg( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
00:00:07.980 - Primitive: CPHY_RL_Setup_REQ Send event:[3] CPHY ! CPHY_RL_Setup_REQ = PDU (view PDU) 00:00:07.990 - Primitive: CPHY_RL_Setup_CNF begin "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF Receive event:[4] CPHY ? CPHY_RL_Setup_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 0 ]} 00:00:07.990 - Primitive: CPHY_RL_Setup_REQ Send event:[5] CPHY ! CPHY_RL_Setup_REQ = PDU (view PDU) 00:00:08.030 - Primitive: CPHY_RL_Setup_CNF begin "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF Receive event:[6] CPHY ? CPHY_RL_Setup_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 1 ]} 00:00:08.030 - Primitive: CPHY_RL_Setup_REQ Send event:[7] CPHY ! CPHY_RL_Setup_REQ = PDU (view PDU) 00:00:08.040 - Primitive: CPHY_RL_Setup_CNF begin "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF Receive event:[8] CPHY ? CPHY_RL_Setup_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 2 ]} 00:00:08.040 - Primitive: CPHY_RL_Setup_REQ Send event:[9] CPHY ! CPHY_RL_Setup_REQ = PDU (view PDU) 00:00:08.060 - Primitive: CPHY_RL_Setup_CNF begin "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF Receive event:[10] CPHY ? CPHY_RL_Setup_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 4 ]} 00:00:08.060 - Primitive: CPHY_TrCH_Config_REQ Send event:[11] CPHY ! CPHY_TrCH_Config_REQ = PDU (view PDU) 00:00:08.260 - Primitive: CPHY_TrCH_Config_CNF begin "ca_TrChCfgCnf" of type CPHY_TrCH_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_TrChCfgCnf" of type CPHY_TrCH_Config_CNF Receive event:[12] CPHY ? CPHY_TrCH_Config_CNF = PDU (view PDU) 00:00:08.260 - Primitive: CMAC_Config_REQ Send event:[13] CMAC ! CMAC_Config_REQ = PDU (view PDU) 00:00:08.290 - Primitive: CMAC_Config_CNF begin "ca_CMAC_CfgCnf" of type CMAC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_CfgCnf" of type CMAC_Config_CNF Receive event:[14] CMAC ? CMAC_Config_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 4 ]} Attach:[2] Exit Test Step ts_SS_BCH_SCH_CPICH_Cfg
Attach:[3] Enter Test Step ts_SS_PCH_FACH_CCCH_Cfg( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
00:00:08.290 - Primitive: CPHY_RL_Setup_REQ Send event:[3] CPHY ! CPHY_RL_Setup_REQ = PDU (view PDU) 00:00:08.310 - Primitive: CPHY_RL_Setup_CNF begin "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 5 against 5 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF Receive event:[4] CPHY ? CPHY_RL_Setup_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 5 ]} 00:00:08.310 - Primitive: CPHY_TrCH_Config_REQ Send event:[5] CPHY ! CPHY_TrCH_Config_REQ = PDU (view PDU) 00:00:08.340 - Primitive: CPHY_TrCH_Config_CNF begin "ca_TrChCfgCnf" of type CPHY_TrCH_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 5 against 5 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_TrChCfgCnf" of type CPHY_TrCH_Config_CNF Receive event:[6] CPHY ? CPHY_TrCH_Config_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 5 ]} 00:00:08.340 - Primitive: CMAC_Config_REQ Send event:[7] CMAC ! CMAC_Config_REQ = PDU (view PDU) 00:00:08.350 - Primitive: CMAC_Config_CNF begin "ca_CMAC_CfgCnf" of type CMAC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 5 against 5 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_CfgCnf" of type CMAC_Config_CNF Receive event:[8] CMAC ? CMAC_Config_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 5 ]} 00:00:08.350 - Primitive: CPHY_RL_Setup_REQ Send event:[9] CPHY ! CPHY_RL_Setup_REQ = PDU (view PDU) 00:00:08.370 - Primitive: CPHY_RL_Setup_CNF begin "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF Receive event:[10] CPHY ? CPHY_RL_Setup_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 6 ]} Attach:[3] Exit Test Step ts_SS_PCH_FACH_CCCH_Cfg
Attach:[4] Enter Test Step ts_SS_RACH_CCCH_Cfg( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
00:00:08.370 - Primitive: CPHY_RL_Setup_REQ Send event:[3] CPHY ! CPHY_RL_Setup_REQ = PDU (view PDU) 00:00:08.380 - Primitive: CPHY_RL_Setup_CNF begin "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 7 against 7 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF Receive event:[4] CPHY ? CPHY_RL_Setup_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 7 ]} 00:00:08.380 - Primitive: CPHY_RL_Setup_REQ Send event:[5] CPHY ! CPHY_RL_Setup_REQ = PDU (view PDU) 00:00:08.400 - Primitive: CPHY_RL_Setup_CNF begin "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 8 against 8 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF Receive event:[6] CPHY ? CPHY_RL_Setup_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 8 ]} 00:00:08.400 - Primitive: CPHY_TrCH_Config_REQ Send event:[7] CPHY ! CPHY_TrCH_Config_REQ = PDU (view PDU) 00:00:08.450 - Primitive: CPHY_TrCH_Config_CNF begin "ca_TrChCfgCnf" of type CPHY_TrCH_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 8 against 8 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_TrChCfgCnf" of type CPHY_TrCH_Config_CNF Receive event:[8] CPHY ? CPHY_TrCH_Config_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 8 ]} 00:00:08.450 - Primitive: CMAC_Config_REQ Send event:[9] CMAC ! CMAC_Config_REQ = PDU (view PDU) 00:00:08.460 - Primitive: CMAC_Config_CNF begin "ca_CMAC_CfgCnf" of type CMAC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 8 against 8 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_CfgCnf" of type CMAC_Config_CNF Receive event:[10] CMAC ? CMAC_Config_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 8 ]} Attach:[4] Exit Test Step ts_SS_RACH_CCCH_Cfg
Attach:[5] Enter Test Step ts_CountConfiguredCell( )
| Assignment:[1] tcv_NumCfgCell := 0 Attach:[2] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 0 , frequenc ...
| (view Test Step parameters) Attach:[2] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[3] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 1 , frequenc ...
| (view Test Step parameters) Attach:[3] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[4] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 2 , frequenc ...
| (view Test Step parameters) Attach:[4] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[5] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 3 , frequenc ...
| (view Test Step parameters) Attach:[5] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[6] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 4 , frequenc ...
| (view Test Step parameters) Attach:[6] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[7] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 5 , frequenc ...
| (view Test Step parameters) Attach:[7] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[8] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 6 , frequenc ...
| (view Test Step parameters) Attach:[8] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[9] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 7 , frequenc ...
| (view Test Step parameters) Attach:[9] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[5] Exit Test Step ts_CountConfiguredCell
Attach:[7] Enter Test Step ts_SS_1DCH_DCCH_Cfg( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Assignment:[3] tcv_TGCFN := 0 00:00:08.460 - Primitive: CPHY_RL_Setup_REQ Send event:[4] CPHY ! CPHY_RL_Setup_REQ = PDU (view PDU) 00:00:08.490 - Primitive: CPHY_RL_Setup_CNF begin "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 26 against 26 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF Receive event:[5] CPHY ? CPHY_RL_Setup_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 26 ]} 00:00:08.490 - Primitive: CPHY_TrCH_Config_REQ Send event:[6] CPHY ! CPHY_TrCH_Config_REQ = PDU (view PDU) 00:00:08.530 - Primitive: CPHY_TrCH_Config_CNF begin "ca_TrChCfgCnf" of type CPHY_TrCH_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 26 against 26 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_TrChCfgCnf" of type CPHY_TrCH_Config_CNF Receive event:[7] CPHY ? CPHY_TrCH_Config_CNF = PDU (view PDU) 00:00:08.530 - Primitive: CMAC_Config_REQ Send event:[8] CMAC ! CMAC_Config_REQ = PDU (view PDU) 00:00:08.570 - Primitive: CMAC_Config_CNF begin "ca_CMAC_CfgCnf" of type CMAC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 26 against 26 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_CfgCnf" of type CMAC_Config_CNF Receive event:[9] CMAC ? CMAC_Config_CNF = PDU: { cellId: -1 , routingInfo: [physicalChannelIdentity: 26 ]} 00:00:08.570 - Primitive: CPHY_RL_Setup_REQ Send event:[10] CPHY ! CPHY_RL_Setup_REQ = PDU (view PDU) 00:00:08.590 - Primitive: CPHY_RL_Setup_CNF begin "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 20 against 20 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF Receive event:[11] CPHY ? CPHY_RL_Setup_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 20 ]} 00:00:08.590 - Primitive: CPHY_TrCH_Config_REQ Send event:[12] CPHY ! CPHY_TrCH_Config_REQ = PDU (view PDU) 00:00:08.630 - Primitive: CPHY_TrCH_Config_CNF begin "ca_TrChCfgCnf" of type CPHY_TrCH_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 20 against 20 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_TrChCfgCnf" of type CPHY_TrCH_Config_CNF Receive event:[13] CPHY ? CPHY_TrCH_Config_CNF = PDU (view PDU) 00:00:08.630 - Primitive: CMAC_Config_REQ Send event:[14] CMAC ! CMAC_Config_REQ = PDU (view PDU) 00:00:08.670 - Primitive: CMAC_Config_CNF begin "ca_CMAC_CfgCnf" of type CMAC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 20 against 20 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_CfgCnf" of type CMAC_Config_CNF Receive event:[15] CMAC ? CMAC_Config_CNF = PDU: { cellId: -1 , routingInfo: [physicalChannelIdentity: 20 ]} Attach:[7] Exit Test Step ts_SS_1DCH_DCCH_Cfg
Attach:[8] Enter Test Step ts_SS_RB_BCCH_BCH_Cfg( 0 )
| 00:00:08.670 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:00:08.680 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} Attach:[8] Exit Test Step ts_SS_RB_BCCH_BCH_Cfg
Attach:[9] Enter Test Step ts_SS_RB_PCCH_Cfg( 0 )
| 00:00:08.680 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:00:08.700 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -2 against -2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -2 ]} Attach:[9] Exit Test Step ts_SS_RB_PCCH_Cfg
Attach:[10] Enter Test Step ts_SS_RB0_Cfg( 0 )
| 00:00:08.700 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:00:08.710 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: 0 ]} 00:00:08.710 - Primitive: CRLC_Config_REQ Send event:[3] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:00:08.730 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[4] CRLC ? CRLC_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: 0 ]} Attach:[10] Exit Test Step ts_SS_RB0_Cfg
Attach:[11] Enter Test Step ts_SS_RB1_ToRB4_Cfg( )
| 00:00:08.730 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:00:08.740 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 1 ]} 00:00:08.740 - Primitive: CRLC_Config_REQ Send event:[3] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:00:08.780 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[4] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 2 ]} 00:00:08.780 - Primitive: CRLC_Config_REQ Send event:[5] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:00:08.790 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[6] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 3 ]} 00:00:08.790 - Primitive: CRLC_Config_REQ Send event:[7] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:00:08.810 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[8] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 4 ]} Attach:[11] Exit Test Step ts_SS_RB1_ToRB4_Cfg
Assignment:[12] DL_DPCH_SHO := GcTRUE Assignment:[12] UL_DPCH_SHO := GcTRUE Assignment:[12] cellConfig := cell_DCH_StandAloneSRB_NoConn Attach:[13] Enter Test Step ts_SaveCellInfo( 0 )
| Assignment:[2] tcv_CellInfoA := (view Assignment) Attach:[13] Exit Test Step ts_SaveCellInfo
Attach:[1] Exit Test Step ts_SS_CreateCellDCH
Attach:[2] Enter Test Step ts_SendDefSysInfo( 0 )
| Attach:[1] Enter Test Step ts_UTRAN_GERAN_ParaInit( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Assignment:[3] tcv_SIB3 := (view Assignment) Assignment:[3] tcv_SIB4 := (view Assignment) Attach:[1] Exit Test Step ts_UTRAN_GERAN_ParaInit
Attach:[2] Enter Test Step ts_CellDependentPara( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Assignment:[3] cellIdentity := '0000000000000000000000000000'B Assignment:[3] cellIdentity := '0000000000000000000000000000'B Attach:[2] Exit Test Step ts_CellDependentPara
Attach:[3] Enter Test Step ts_InitializeSIB2AndSIB18( { cellId: 0 , frequenc ...
| (view Test Step parameters) Assignment:[1] tcv_SIB2 := { ura_IdentityList: [ '0000000000000001'B ] , nonCriticalExtensions: OMIT} Attach:[5] Enter Test Step ts_InitializeSIB2AndSIB18::lt_Init2PLMN( { cellId: 0 , frequenc ...
| (view Test Step parameters) Assignment:[10] tcv_SIB18 := (view Assignment) Attach:[5] Exit Test Step ts_InitializeSIB2AndSIB18::lt_Init2PLMN
Attach:[3] Exit Test Step ts_InitializeSIB2AndSIB18
Attach:[4] Enter Test Step ts_InitializeSIB11_SIB12( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[5] Enter Test Step ts_InitializeSIB11_SIB12::lt_1Or2PLMN( 0 )
| Assignment:[10] tcv_SIB11 := (view Assignment) Assignment:[10] tcv_SIB12 := (view Assignment) Attach:[5] Exit Test Step ts_InitializeSIB11_SIB12::lt_1Or2PLMN
Attach:[4] Exit Test Step ts_InitializeSIB11_SIB12
Attach:[6] Enter Test Step ts_SendNoSegDefSchedul( 0 )
| Attach:[1] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:08.810 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[1] Exit Test Step ts_Scheduling
00:00:08.820 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[2] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} 00:00:08.820 - Primitive: RLC_TR_DATA_REQ 00:00:08.820 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[3] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[6] Exit Test Step ts_SendNoSegDefSchedul
Attach:[7] Enter Test Step ts_SendSIB1( { cn_CommonGSM_MAP_NAS ...
| (view Test Step parameters) Assignment:[1] tcv_SIB1 := (view Assignment) 00:00:08.820 - Primitive: o_SIB_PER_Encoding Assignment:[1] seg1 := (view Assignment) 00:00:08.820 - Primitive: o_SIB_PER_Encoding Assignment:[1] seg2 := '00000000000000000001'B Attach:[4] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:08.820 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[4] Exit Test Step ts_Scheduling
00:00:08.840 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[5] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} 00:00:08.840 - Primitive: RLC_TR_DATA_REQ 00:00:08.840 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[6] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Assignment:[7] sysInfoType1 := 2 Attach:[8] Enter Test Step ts_ChangeMIB_ValueTag( )
| Attach:[8] Exit Test Step ts_ChangeMIB_ValueTag
Attach:[7] Exit Test Step ts_SendSIB1
Attach:[8] Enter Test Step ts_SendSIB2( { ura_IdentityList: [ ...
| (view Test Step parameters) Assignment:[1] tcv_SIB2 := { ura_IdentityList: [ '0000000000000001'B ] , nonCriticalExtensions: OMIT} 00:00:08.840 - Primitive: o_SIB_PER_Encoding Assignment:[1] seg1 := '00000000000000000001'B 00:00:08.840 - Primitive: o_SIB_PER_Encoding Assignment:[1] seg2 := (view Assignment) Attach:[4] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:08.840 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[4] Exit Test Step ts_Scheduling
00:00:08.850 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[5] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} 00:00:08.850 - Primitive: RLC_TR_DATA_REQ 00:00:08.850 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[6] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Assignment:[7] sysInfoType2 := 2 Attach:[8] Enter Test Step ts_ChangeMIB_ValueTag( )
| Attach:[8] Exit Test Step ts_ChangeMIB_ValueTag
Attach:[8] Exit Test Step ts_SendSIB2
Attach:[9] Enter Test Step ts_SendSIB3( { sib4indicator: GcTRU ...
| (view Test Step parameters) Assignment:[1] tcv_SIB3 := (view Assignment) 00:00:08.850 - Primitive: o_SIB_PER_Encoding Assignment:[1] seg1 := (view Assignment) 00:00:08.850 - Primitive: o_SIB_PER_Encoding Assignment:[1] seg2 := '100000101000000010000001'B Attach:[4] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:08.870 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[4] Exit Test Step ts_Scheduling
00:00:08.880 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[5] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} 00:00:08.880 - Primitive: RLC_TR_DATA_REQ 00:00:08.880 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[6] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Assignment:[7] sysInfoType3 := 2 Attach:[8] Enter Test Step ts_ChangeMIB_ValueTag( )
| Attach:[8] Exit Test Step ts_ChangeMIB_ValueTag
Attach:[9] Exit Test Step ts_SendSIB3
Attach:[10] Enter Test Step ts_SendSIB4( { cellIdentity: '00000 ...
| (view Test Step parameters) Assignment:[1] tcv_SIB4 := (view Assignment) 00:00:08.900 - Primitive: o_SIB_PER_Encoding Assignment:[1] seg1 := (view Assignment) 00:00:08.900 - Primitive: o_SIB_PER_Encoding Assignment:[1] seg2 := '100000101000000010000001'B Attach:[4] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:08.900 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[4] Exit Test Step ts_Scheduling
00:00:08.920 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[5] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} 00:00:08.920 - Primitive: RLC_TR_DATA_REQ 00:00:08.920 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[6] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Assignment:[7] sysInfoType4 := 2 Attach:[8] Enter Test Step ts_ChangeMIB_ValueTag( )
| Attach:[8] Exit Test Step ts_ChangeMIB_ValueTag
Attach:[10] Exit Test Step ts_SendSIB4
Attach:[11] Enter Test Step ts_SendSIB5( { sib6indicator: GcTRU ...
| (view Test Step parameters) 00:00:08.950 - Primitive: o_SIB_PER_Encoding Assignment:[1] tcv_Segs := (view Assignment) Assignment:[38] sysInfoType5 := 2 Assignment:[38] scheduling := (view Assignment) Attach:[39] Enter Test Step ts_ChangeMIB_ValueTag( )
| Attach:[39] Exit Test Step ts_ChangeMIB_ValueTag
Attach:[40] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:08.980 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[40] Exit Test Step ts_Scheduling
00:00:08.990 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[41] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} 00:00:08.990 - Primitive: RLC_TR_DATA_REQ 00:00:08.990 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[42] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[43] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:08.990 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[43] Exit Test Step ts_Scheduling
00:00:09.010 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[44] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} 00:00:09.010 - Primitive: RLC_TR_DATA_REQ 00:00:09.010 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[45] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[46] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:09.010 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[46] Exit Test Step ts_Scheduling
00:00:09.030 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[47] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} 00:00:09.030 - Primitive: RLC_TR_DATA_REQ 00:00:09.030 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[48] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[49] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:09.030 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[49] Exit Test Step ts_Scheduling
00:00:09.040 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[50] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} 00:00:09.040 - Primitive: RLC_TR_DATA_REQ 00:00:09.040 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[52] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[11] Exit Test Step ts_SendSIB5
Attach:[12] Enter Test Step ts_SendSIB6( { pich_PowerOffset: -5 ...
| (view Test Step parameters) 00:00:09.040 - Primitive: o_SIB_PER_Encoding Assignment:[1] tcv_Segs := (view Assignment) Assignment:[5] sysInfoType6 := 2 Assignment:[5] scheduling := { scheduling: { segCount: OMIT, sib_Pos: [rep64: 3 ], sib_PosOffsetInfo: OMIT} } Attach:[6] Enter Test Step ts_ChangeSB1_ValueTag( )
| Assignment:[2] tcv_SB1_ValueTag := 2 Assignment:[2] sysInfoTypeSB1 := 2 Assignment:[2] tcv_SB1_ValueTagChanged := GcTRUE Attach:[3] Enter Test Step ts_ChangeMIB_ValueTag( )
| Attach:[3] Exit Test Step ts_ChangeMIB_ValueTag
Attach:[6] Exit Test Step ts_ChangeSB1_ValueTag
Attach:[7] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:09.040 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[7] Exit Test Step ts_Scheduling
00:00:09.060 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[8] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} Attach:[9] Enter Test Step ts_SendSIB6::lt_CompleteSIB( systemInformationBlockType6 )
| 00:00:09.060 - Primitive: RLC_TR_DATA_REQ 00:00:09.060 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[76] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[9] Exit Test Step ts_SendSIB6::lt_CompleteSIB
Attach:[10] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:09.060 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[10] Exit Test Step ts_Scheduling
00:00:09.070 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[11] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} 00:00:09.070 - Primitive: RLC_TR_DATA_REQ 00:00:09.070 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[12] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[13] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:09.070 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[13] Exit Test Step ts_Scheduling
00:00:09.090 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[14] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} 00:00:09.090 - Primitive: RLC_TR_DATA_REQ 00:00:09.090 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[15] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[16] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:09.090 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[16] Exit Test Step ts_Scheduling
00:00:09.100 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[17] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} 00:00:09.100 - Primitive: RLC_TR_DATA_REQ 00:00:09.100 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[18] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[12] Exit Test Step ts_SendSIB6
Attach:[13] Enter Test Step ts_SendSIB7( { modeSpecificInfo: [f ...
| (view Test Step parameters) 00:00:09.100 - Primitive: o_SIB_PER_Encoding Assignment:[1] tcv_Segs := (view Assignment) Assignment:[1] tcv_SIB7 := (view Assignment) Attach:[4] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:09.100 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[4] Exit Test Step ts_Scheduling
00:00:09.120 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[5] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} Attach:[6] Enter Test Step ts_SendSIB7::lt_CompleteSIB( systemInformationBlockType7 )
| 00:00:09.120 - Primitive: RLC_TR_DATA_REQ 00:00:09.120 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[13] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[6] Exit Test Step ts_SendSIB7::lt_CompleteSIB
Attach:[7] Enter Test Step ts_SendSIB7::lt_ConcatWithSIB3( { modeSpecificInfo: [f ...
| (view Test Step parameters) 00:00:09.120 - Primitive: o_SIB_PER_Encoding Assignment:[14] seg1 := '100000101000000010000001'B 00:00:09.120 - Primitive: o_SIB_PER_Encoding Assignment:[14] seg2 := (view Assignment) Attach:[17] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:09.120 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[17] Exit Test Step ts_Scheduling
00:00:09.130 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[18] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} 00:00:09.130 - Primitive: RLC_TR_DATA_REQ 00:00:09.130 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[19] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[7] Exit Test Step ts_SendSIB7::lt_ConcatWithSIB3
Attach:[8] Enter Test Step ts_SendSIB7::lt_ConcatWithSIB18( { modeSpecificInfo: [f ...
| (view Test Step parameters) 00:00:09.130 - Primitive: o_SIB_PER_Encoding Assignment:[20] seg2 := '100010000001000000000010000000001'B Attach:[23] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:09.130 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[23] Exit Test Step ts_Scheduling
00:00:09.150 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[24] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} 00:00:09.150 - Primitive: RLC_TR_DATA_REQ 00:00:09.150 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[25] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[8] Exit Test Step ts_SendSIB7::lt_ConcatWithSIB18
Attach:[9] Enter Test Step ts_SendSIB7::lt_ConcatWithSIB4( { modeSpecificInfo: [f ...
| (view Test Step parameters) 00:00:09.150 - Primitive: o_SIB_PER_Encoding Assignment:[26] seg2 := (view Assignment) Attach:[29] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:09.150 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[29] Exit Test Step ts_Scheduling
00:00:09.170 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[30] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} 00:00:09.170 - Primitive: RLC_TR_DATA_REQ 00:00:09.170 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[31] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[9] Exit Test Step ts_SendSIB7::lt_ConcatWithSIB4
Attach:[13] Exit Test Step ts_SendSIB7
Attach:[14] Enter Test Step ts_SendSIB11( { sib12indicator: GcTR ...
| (view Test Step parameters) 00:00:09.210 - Primitive: o_SIB_PER_Encoding Assignment:[1] tcv_Segs := (view Assignment) Assignment:[17] sysInfoType11 := 2 Assignment:[17] scheduling := (view Assignment) Attach:[18] Enter Test Step ts_ChangeSB1_ValueTag( )
| Attach:[18] Exit Test Step ts_ChangeSB1_ValueTag
Attach:[19] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:09.230 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[19] Exit Test Step ts_Scheduling
00:00:09.240 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[20] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} 00:00:09.240 - Primitive: RLC_TR_DATA_REQ 00:00:09.240 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[21] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[22] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:09.240 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[22] Exit Test Step ts_Scheduling
00:00:09.260 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[23] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} 00:00:09.260 - Primitive: RLC_TR_DATA_REQ 00:00:09.260 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[24] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[25] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:09.260 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[25] Exit Test Step ts_Scheduling
00:00:09.280 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[26] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} 00:00:09.280 - Primitive: RLC_TR_DATA_REQ 00:00:09.280 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[28] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[14] Exit Test Step ts_SendSIB11
Attach:[15] Enter Test Step ts_SendSIB12( { fach_MeasurementOcca ...
| (view Test Step parameters) 00:00:09.280 - Primitive: o_SIB_PER_Encoding Assignment:[1] tcv_Segs := (view Assignment) Assignment:[5] sysInfoType12 := 2 Assignment:[5] scheduling := { scheduling: { segCount: OMIT, sib_Pos: [rep64: 13 ], sib_PosOffsetInfo: OMIT} } Attach:[6] Enter Test Step ts_ChangeSB1_ValueTag( )
| Attach:[6] Exit Test Step ts_ChangeSB1_ValueTag
Attach:[7] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:09.280 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[7] Exit Test Step ts_Scheduling
00:00:09.290 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[8] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} Attach:[9] Enter Test Step ts_SendSIB12::lt_CompleteSIB( systemInformationBlockType12 )
| 00:00:09.290 - Primitive: RLC_TR_DATA_REQ 00:00:09.290 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[50] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[9] Exit Test Step ts_SendSIB12::lt_CompleteSIB
Attach:[10] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:09.290 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[10] Exit Test Step ts_Scheduling
00:00:09.310 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[11] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} 00:00:09.310 - Primitive: RLC_TR_DATA_REQ 00:00:09.310 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[12] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[13] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:09.310 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[13] Exit Test Step ts_Scheduling
00:00:09.320 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[14] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} 00:00:09.320 - Primitive: RLC_TR_DATA_REQ 00:00:09.320 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[15] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[15] Exit Test Step ts_SendSIB12
Attach:[16] Enter Test Step ts_SendSIB18( { idleModePLMNIdentiti ...
| (view Test Step parameters) Assignment:[1] tcv_SIB18 := (view Assignment) 00:00:09.320 - Primitive: o_SIB_PER_Encoding Assignment:[1] seg1 := '100010000001000000000010000000001'B 00:00:09.320 - Primitive: o_SIB_PER_Encoding Assignment:[1] seg2 := '100000101000000010000001'B Attach:[4] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:09.320 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[4] Exit Test Step ts_Scheduling
00:00:09.340 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[5] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} 00:00:09.340 - Primitive: RLC_TR_DATA_REQ 00:00:09.340 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[6] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Assignment:[7] sysInfoType18 := 2 Attach:[8] Enter Test Step ts_ChangeSB1_ValueTag( )
| Attach:[8] Exit Test Step ts_ChangeSB1_ValueTag
Attach:[16] Exit Test Step ts_SendSIB18
Attach:[17] Enter Test Step ts_SendSB1_DefSchedul( { sib_ReferenceList: [ ...
| (view Test Step parameters) 00:00:09.340 - Primitive: o_SIB_PER_Encoding Assignment:[1] tcv_Segs := (view Assignment) Attach:[3] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:09.350 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[3] Exit Test Step ts_Scheduling
00:00:09.370 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[4] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} Attach:[5] Enter Test Step ts_SendSB1_DefSchedul::lt_CompleteSIB( schedulingBlock1 )
| 00:00:09.370 - Primitive: RLC_TR_DATA_REQ 00:00:09.370 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[12] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[5] Exit Test Step ts_SendSB1_DefSchedul::lt_CompleteSIB
Attach:[6] Enter Test Step ts_ChangeSB1_ValueTag( )
| Attach:[6] Exit Test Step ts_ChangeSB1_ValueTag
Assignment:[7] scheduling := { scheduling: { segCount: OMIT, sib_Pos: [rep16: 1 ], sib_PosOffsetInfo: OMIT} } Assignment:[7] tcv_SB1_ValueTagChanged := GcFALSE Attach:[17] Exit Test Step ts_SendSB1_DefSchedul
Attach:[18] Enter Test Step ts_SendMIB( { mib_ValueTag: 1 , pl ...
| (view Test Step parameters) Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Assignment:[2] mcc := [ 0 , 0 , 1 ] Assignment:[2] mnc := [ 0 , 1 ] 00:00:09.370 - Primitive: o_SIB_PER_Encoding Assignment:[3] tcv_Segs := (view Assignment) Attach:[6] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:09.370 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[6] Exit Test Step ts_Scheduling
00:00:09.380 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[7] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} Attach:[8] Enter Test Step ts_SendMIB::lt_CompleteSIB( masterInformationBlock )
| 00:00:09.400 - Primitive: RLC_TR_DATA_REQ 00:00:09.400 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[13] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[8] Exit Test Step ts_SendMIB::lt_CompleteSIB
Assignment:[9] tcv_MIB_ValueTagChanged := GcFALSE Attach:[18] Exit Test Step ts_SendMIB
Attach:[2] Exit Test Step ts_SendDefSysInfo
Attach:[3] Enter Test Step ts_SS_CreateCellDCH( 1 )
| Attach:[1] Enter Test Step ts_SS_CellCfg( 1 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 1 )
| Assignment:[4] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[4] Enter Test Step ts_SS_CellCfg::lt_CelllsAlreadyStarted( 1 )
| Attach:[11] Enter Test Step ts_CountConfiguredCell( )
| Assignment:[1] tcv_NumCfgCell := 0 Attach:[2] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 0 , frequenc ...
| (view Test Step parameters) Assignment:[11] tcv_NumCfgCell := 1 Attach:[2] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[3] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 1 , frequenc ...
| (view Test Step parameters) Attach:[3] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[4] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 2 , frequenc ...
| (view Test Step parameters) Attach:[4] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[5] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 3 , frequenc ...
| (view Test Step parameters) Attach:[5] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[6] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 4 , frequenc ...
| (view Test Step parameters) Attach:[6] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[7] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 5 , frequenc ...
| (view Test Step parameters) Attach:[7] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[8] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 6 , frequenc ...
| (view Test Step parameters) Attach:[8] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[9] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 7 , frequenc ...
| (view Test Step parameters) Attach:[9] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[11] Exit Test Step ts_CountConfiguredCell
Attach:[4] Exit Test Step ts_SS_CellCfg::lt_CelllsAlreadyStarted
00:00:09.400 - Primitive: CPHY_Cell_Config_REQ Send event:[6] CPHY ! CPHY_Cell_Config_REQ = PDU (view PDU) 00:00:09.540 - Primitive: CPHY_Cell_Config_CNF begin "ca_CellCfgCnf" of type CPHY_Cell_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "cellId" of type INTEGER end "ca_CellCfgCnf" of type CPHY_Cell_Config_CNF Receive event:[7] CPHY ? CPHY_Cell_Config_CNF = PDU: { cellId: 1 } Attach:[8] Enter Test Step ts_SaveCellInfo( 1 )
| Assignment:[4] tcv_CellInfoB := (view Assignment) Attach:[8] Exit Test Step ts_SaveCellInfo
Attach:[1] Exit Test Step ts_SS_CellCfg
Attach:[2] Enter Test Step ts_SS_BCH_SCH_CPICH_Cfg( 1 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 1 )
| Assignment:[4] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
00:00:09.540 - Primitive: CPHY_RL_Setup_REQ Send event:[3] CPHY ! CPHY_RL_Setup_REQ = PDU (view PDU) 00:00:09.560 - Primitive: CPHY_RL_Setup_CNF begin "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF Receive event:[4] CPHY ? CPHY_RL_Setup_CNF = PDU: { cellId: 1 , routingInfo: [physicalChannelIdentity: 0 ]} 00:00:09.560 - Primitive: CPHY_RL_Setup_REQ Send event:[5] CPHY ! CPHY_RL_Setup_REQ = PDU (view PDU) 00:00:09.570 - Primitive: CPHY_RL_Setup_CNF begin "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF Receive event:[6] CPHY ? CPHY_RL_Setup_CNF = PDU: { cellId: 1 , routingInfo: [physicalChannelIdentity: 1 ]} 00:00:09.570 - Primitive: CPHY_RL_Setup_REQ Send event:[7] CPHY ! CPHY_RL_Setup_REQ = PDU (view PDU) 00:00:09.590 - Primitive: CPHY_RL_Setup_CNF begin "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF Receive event:[8] CPHY ? CPHY_RL_Setup_CNF = PDU: { cellId: 1 , routingInfo: [physicalChannelIdentity: 2 ]} 00:00:09.590 - Primitive: CPHY_RL_Setup_REQ Send event:[9] CPHY ! CPHY_RL_Setup_REQ = PDU (view PDU) 00:00:09.600 - Primitive: CPHY_RL_Setup_CNF begin "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF Receive event:[10] CPHY ? CPHY_RL_Setup_CNF = PDU: { cellId: 1 , routingInfo: [physicalChannelIdentity: 4 ]} 00:00:09.600 - Primitive: CPHY_TrCH_Config_REQ Send event:[11] CPHY ! CPHY_TrCH_Config_REQ = PDU (view PDU) 00:00:09.630 - Primitive: CPHY_TrCH_Config_CNF begin "ca_TrChCfgCnf" of type CPHY_TrCH_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_TrChCfgCnf" of type CPHY_TrCH_Config_CNF Receive event:[12] CPHY ? CPHY_TrCH_Config_CNF = PDU (view PDU) 00:00:09.630 - Primitive: CMAC_Config_REQ Send event:[13] CMAC ! CMAC_Config_REQ = PDU (view PDU) 00:00:09.650 - Primitive: CMAC_Config_CNF begin "ca_CMAC_CfgCnf" of type CMAC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_CfgCnf" of type CMAC_Config_CNF Receive event:[14] CMAC ? CMAC_Config_CNF = PDU: { cellId: 1 , routingInfo: [physicalChannelIdentity: 4 ]} Attach:[2] Exit Test Step ts_SS_BCH_SCH_CPICH_Cfg
Attach:[3] Enter Test Step ts_SS_PCH_FACH_CCCH_Cfg( 1 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 1 )
| Assignment:[4] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
00:00:09.650 - Primitive: CPHY_RL_Setup_REQ Send event:[3] CPHY ! CPHY_RL_Setup_REQ = PDU (view PDU) 00:00:09.670 - Primitive: CPHY_RL_Setup_CNF begin "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 5 against 5 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF Receive event:[4] CPHY ? CPHY_RL_Setup_CNF = PDU: { cellId: 1 , routingInfo: [physicalChannelIdentity: 5 ]} 00:00:09.670 - Primitive: CPHY_TrCH_Config_REQ Send event:[5] CPHY ! CPHY_TrCH_Config_REQ = PDU (view PDU) 00:00:09.700 - Primitive: CPHY_TrCH_Config_CNF begin "ca_TrChCfgCnf" of type CPHY_TrCH_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 5 against 5 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_TrChCfgCnf" of type CPHY_TrCH_Config_CNF Receive event:[6] CPHY ? CPHY_TrCH_Config_CNF = PDU: { cellId: 1 , routingInfo: [physicalChannelIdentity: 5 ]} 00:00:09.700 - Primitive: CMAC_Config_REQ Send event:[7] CMAC ! CMAC_Config_REQ = PDU (view PDU) 00:00:09.710 - Primitive: CMAC_Config_CNF begin "ca_CMAC_CfgCnf" of type CMAC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 5 against 5 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_CfgCnf" of type CMAC_Config_CNF Receive event:[8] CMAC ? CMAC_Config_CNF = PDU: { cellId: 1 , routingInfo: [physicalChannelIdentity: 5 ]} 00:00:09.710 - Primitive: CPHY_RL_Setup_REQ Send event:[9] CPHY ! CPHY_RL_Setup_REQ = PDU (view PDU) 00:00:09.730 - Primitive: CPHY_RL_Setup_CNF begin "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF Receive event:[10] CPHY ? CPHY_RL_Setup_CNF = PDU: { cellId: 1 , routingInfo: [physicalChannelIdentity: 6 ]} Attach:[3] Exit Test Step ts_SS_PCH_FACH_CCCH_Cfg
Attach:[4] Enter Test Step ts_SS_RACH_CCCH_Cfg( 1 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 1 )
| Assignment:[4] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
00:00:09.730 - Primitive: CPHY_RL_Setup_REQ Send event:[3] CPHY ! CPHY_RL_Setup_REQ = PDU (view PDU) 00:00:09.740 - Primitive: CPHY_RL_Setup_CNF begin "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 7 against 7 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF Receive event:[4] CPHY ? CPHY_RL_Setup_CNF = PDU: { cellId: 1 , routingInfo: [physicalChannelIdentity: 7 ]} 00:00:09.740 - Primitive: CPHY_RL_Setup_REQ Send event:[5] CPHY ! CPHY_RL_Setup_REQ = PDU (view PDU) 00:00:09.760 - Primitive: CPHY_RL_Setup_CNF begin "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 8 against 8 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF Receive event:[6] CPHY ? CPHY_RL_Setup_CNF = PDU: { cellId: 1 , routingInfo: [physicalChannelIdentity: 8 ]} 00:00:09.760 - Primitive: CPHY_TrCH_Config_REQ Send event:[7] CPHY ! CPHY_TrCH_Config_REQ = PDU (view PDU) 00:00:09.810 - Primitive: CPHY_TrCH_Config_CNF begin "ca_TrChCfgCnf" of type CPHY_TrCH_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 8 against 8 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_TrChCfgCnf" of type CPHY_TrCH_Config_CNF Receive event:[8] CPHY ? CPHY_TrCH_Config_CNF = PDU: { cellId: 1 , routingInfo: [physicalChannelIdentity: 8 ]} 00:00:09.810 - Primitive: CMAC_Config_REQ Send event:[9] CMAC ! CMAC_Config_REQ = PDU (view PDU) 00:00:09.820 - Primitive: CMAC_Config_CNF begin "ca_CMAC_CfgCnf" of type CMAC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 8 against 8 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_CfgCnf" of type CMAC_Config_CNF Receive event:[10] CMAC ? CMAC_Config_CNF = PDU: { cellId: 1 , routingInfo: [physicalChannelIdentity: 8 ]} Attach:[4] Exit Test Step ts_SS_RACH_CCCH_Cfg
Attach:[5] Enter Test Step ts_CountConfiguredCell( )
| Assignment:[1] tcv_NumCfgCell := 0 Attach:[2] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 0 , frequenc ...
| (view Test Step parameters) Assignment:[11] tcv_NumCfgCell := 1 Attach:[2] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[3] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 1 , frequenc ...
| (view Test Step parameters) Attach:[3] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[4] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 2 , frequenc ...
| (view Test Step parameters) Attach:[4] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[5] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 3 , frequenc ...
| (view Test Step parameters) Attach:[5] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[6] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 4 , frequenc ...
| (view Test Step parameters) Attach:[6] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[7] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 5 , frequenc ...
| (view Test Step parameters) Attach:[7] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[8] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 6 , frequenc ...
| (view Test Step parameters) Attach:[8] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[9] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 7 , frequenc ...
| (view Test Step parameters) Attach:[9] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[5] Exit Test Step ts_CountConfiguredCell
Attach:[15] Enter Test Step ts_SS_RB_BCCH_BCH_Cfg( 1 )
| 00:00:09.820 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:00:09.840 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: 1 , routingInfo: [rB_Identity: -1 ]} Attach:[15] Exit Test Step ts_SS_RB_BCCH_BCH_Cfg
Attach:[16] Enter Test Step ts_SS_RB_PCCH_Cfg( 1 )
| 00:00:09.840 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:00:09.850 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -2 against -2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: 1 , routingInfo: [rB_Identity: -2 ]} Attach:[16] Exit Test Step ts_SS_RB_PCCH_Cfg
Attach:[17] Enter Test Step ts_SS_RB0_Cfg( 1 )
| 00:00:09.850 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:00:09.870 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: 1 , routingInfo: [rB_Identity: 0 ]} 00:00:09.870 - Primitive: CRLC_Config_REQ Send event:[3] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:00:09.880 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[4] CRLC ? CRLC_Config_CNF = PDU: { cellId: 1 , routingInfo: [rB_Identity: 0 ]} Attach:[17] Exit Test Step ts_SS_RB0_Cfg
Attach:[18] Enter Test Step ts_SetCellCfg( 1 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 1 )
| Assignment:[4] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Assignment:[2] cellConfig := cell_NoDPCH Attach:[3] Enter Test Step ts_SaveCellInfo( 1 )
| Assignment:[4] tcv_CellInfoB := (view Assignment) Attach:[3] Exit Test Step ts_SaveCellInfo
Attach:[18] Exit Test Step ts_SetCellCfg
Attach:[3] Exit Test Step ts_SS_CreateCellDCH
Attach:[4] Enter Test Step ts_SendDefSysInfo( 1 )
| Attach:[1] Enter Test Step ts_UTRAN_GERAN_ParaInit( 1 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 1 )
| Assignment:[4] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Assignment:[3] tcv_SIB3 := (view Assignment) Assignment:[3] tcv_SIB4 := (view Assignment) Attach:[1] Exit Test Step ts_UTRAN_GERAN_ParaInit
Attach:[2] Enter Test Step ts_CellDependentPara( 1 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 1 )
| Assignment:[4] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Assignment:[5] cellIdentity := '0000000000000000000000000001'B Assignment:[5] cellIdentity := '0000000000000000000000000001'B Attach:[2] Exit Test Step ts_CellDependentPara
Attach:[3] Enter Test Step ts_InitializeSIB2AndSIB18( { cellId: 1 , frequenc ...
| (view Test Step parameters) Assignment:[1] tcv_SIB2 := { ura_IdentityList: [ '0000000000000001'B ] , nonCriticalExtensions: OMIT} Attach:[5] Enter Test Step ts_InitializeSIB2AndSIB18::lt_Init2PLMN( { cellId: 1 , frequenc ...
| (view Test Step parameters) Assignment:[10] tcv_SIB18 := (view Assignment) Attach:[5] Exit Test Step ts_InitializeSIB2AndSIB18::lt_Init2PLMN
Attach:[3] Exit Test Step ts_InitializeSIB2AndSIB18
Attach:[4] Enter Test Step ts_InitializeSIB11_SIB12( 1 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 1 )
| Assignment:[4] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[5] Enter Test Step ts_InitializeSIB11_SIB12::lt_1Or2PLMN( 1 )
| Assignment:[12] tcv_SIB11 := (view Assignment) Assignment:[12] tcv_SIB12 := (view Assignment) Attach:[5] Exit Test Step ts_InitializeSIB11_SIB12::lt_1Or2PLMN
Attach:[4] Exit Test Step ts_InitializeSIB11_SIB12
Attach:[6] Enter Test Step ts_SendNoSegDefSchedul( 1 )
| Attach:[1] Enter Test Step ts_Scheduling( 1 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:09.880 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[1] Exit Test Step ts_Scheduling
00:00:09.900 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[2] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 1 , routingInfo: [rB_Identity: -1 ]} 00:00:09.900 - Primitive: RLC_TR_DATA_REQ 00:00:09.900 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[3] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[6] Exit Test Step ts_SendNoSegDefSchedul
Attach:[7] Enter Test Step ts_SendSIB1( { cn_CommonGSM_MAP_NAS ...
| (view Test Step parameters) Assignment:[1] tcv_SIB1 := (view Assignment) 00:00:09.900 - Primitive: o_SIB_PER_Encoding Assignment:[1] seg1 := (view Assignment) 00:00:09.900 - Primitive: o_SIB_PER_Encoding Assignment:[1] seg2 := '00000000000000000001'B Attach:[4] Enter Test Step ts_Scheduling( 1 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:09.900 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[4] Exit Test Step ts_Scheduling
00:00:09.920 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[5] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 1 , routingInfo: [rB_Identity: -1 ]} 00:00:09.920 - Primitive: RLC_TR_DATA_REQ 00:00:09.920 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[6] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Assignment:[7] sysInfoType1 := 3 Attach:[8] Enter Test Step ts_ChangeMIB_ValueTag( )
| Assignment:[2] mib_ValueTag := 2 Assignment:[2] tcv_MIB_ValueTagChanged := GcTRUE Attach:[8] Exit Test Step ts_ChangeMIB_ValueTag
Attach:[7] Exit Test Step ts_SendSIB1
Attach:[8] Enter Test Step ts_SendSIB2( { ura_IdentityList: [ ...
| (view Test Step parameters) Assignment:[1] tcv_SIB2 := { ura_IdentityList: [ '0000000000000001'B ] , nonCriticalExtensions: OMIT} 00:00:09.920 - Primitive: o_SIB_PER_Encoding Assignment:[1] seg1 := '00000000000000000001'B 00:00:09.920 - Primitive: o_SIB_PER_Encoding Assignment:[1] seg2 := (view Assignment) Attach:[4] Enter Test Step ts_Scheduling( 1 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:09.920 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[4] Exit Test Step ts_Scheduling
00:00:09.930 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[5] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 1 , routingInfo: [rB_Identity: -1 ]} 00:00:09.930 - Primitive: RLC_TR_DATA_REQ 00:00:09.930 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[6] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Assignment:[7] sysInfoType2 := 3 Attach:[8] Enter Test Step ts_ChangeMIB_ValueTag( )
| Attach:[8] Exit Test Step ts_ChangeMIB_ValueTag
Attach:[8] Exit Test Step ts_SendSIB2
Attach:[9] Enter Test Step ts_SendSIB3( { sib4indicator: GcTRU ...
| (view Test Step parameters) Assignment:[1] tcv_SIB3 := (view Assignment) 00:00:09.930 - Primitive: o_SIB_PER_Encoding Assignment:[1] seg1 := (view Assignment) 00:00:09.930 - Primitive: o_SIB_PER_Encoding Assignment:[1] seg2 := '100000101000000010000001'B Attach:[4] Enter Test Step ts_Scheduling( 1 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:09.950 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[4] Exit Test Step ts_Scheduling
00:00:09.960 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[5] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 1 , routingInfo: [rB_Identity: -1 ]} 00:00:09.960 - Primitive: RLC_TR_DATA_REQ 00:00:09.960 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[6] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Assignment:[7] sysInfoType3 := 3 Attach:[8] Enter Test Step ts_ChangeMIB_ValueTag( )
| Attach:[8] Exit Test Step ts_ChangeMIB_ValueTag
Attach:[9] Exit Test Step ts_SendSIB3
Attach:[10] Enter Test Step ts_SendSIB4( { cellIdentity: '00000 ...
| (view Test Step parameters) Assignment:[1] tcv_SIB4 := (view Assignment) 00:00:09.960 - Primitive: o_SIB_PER_Encoding Assignment:[1] seg1 := (view Assignment) 00:00:09.960 - Primitive: o_SIB_PER_Encoding Assignment:[1] seg2 := '100000101000000010000001'B Attach:[4] Enter Test Step ts_Scheduling( 1 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:09.960 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[4] Exit Test Step ts_Scheduling
00:00:09.980 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[5] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 1 , routingInfo: [rB_Identity: -1 ]} 00:00:09.980 - Primitive: RLC_TR_DATA_REQ 00:00:09.980 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[6] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Assignment:[7] sysInfoType4 := 3 Attach:[8] Enter Test Step ts_ChangeMIB_ValueTag( )
| Attach:[8] Exit Test Step ts_ChangeMIB_ValueTag
Attach:[10] Exit Test Step ts_SendSIB4
Attach:[11] Enter Test Step ts_SendSIB5( { sib6indicator: GcTRU ...
| (view Test Step parameters) 00:00:10.030 - Primitive: o_SIB_PER_Encoding Assignment:[1] tcv_Segs := (view Assignment) Assignment:[38] sysInfoType5 := 3 Assignment:[38] scheduling := (view Assignment) Attach:[39] Enter Test Step ts_ChangeMIB_ValueTag( )
| Attach:[39] Exit Test Step ts_ChangeMIB_ValueTag
Attach:[40] Enter Test Step ts_Scheduling( 1 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:10.060 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[40] Exit Test Step ts_Scheduling
00:00:10.070 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[41] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 1 , routingInfo: [rB_Identity: -1 ]} 00:00:10.070 - Primitive: RLC_TR_DATA_REQ 00:00:10.070 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[42] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[43] Enter Test Step ts_Scheduling( 1 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:10.070 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[43] Exit Test Step ts_Scheduling
00:00:10.090 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[44] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 1 , routingInfo: [rB_Identity: -1 ]} 00:00:10.090 - Primitive: RLC_TR_DATA_REQ 00:00:10.090 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[45] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[46] Enter Test Step ts_Scheduling( 1 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:10.090 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[46] Exit Test Step ts_Scheduling
00:00:10.100 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[47] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 1 , routingInfo: [rB_Identity: -1 ]} 00:00:10.100 - Primitive: RLC_TR_DATA_REQ 00:00:10.100 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[48] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[49] Enter Test Step ts_Scheduling( 1 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:10.100 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[49] Exit Test Step ts_Scheduling
00:00:10.120 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[50] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 1 , routingInfo: [rB_Identity: -1 ]} 00:00:10.120 - Primitive: RLC_TR_DATA_REQ 00:00:10.120 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[52] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[11] Exit Test Step ts_SendSIB5
Attach:[12] Enter Test Step ts_SendSIB6( { pich_PowerOffset: -5 ...
| (view Test Step parameters) 00:00:10.120 - Primitive: o_SIB_PER_Encoding Assignment:[1] tcv_Segs := (view Assignment) Assignment:[5] sysInfoType6 := 3 Assignment:[5] scheduling := { scheduling: { segCount: OMIT, sib_Pos: [rep64: 3 ], sib_PosOffsetInfo: OMIT} } Attach:[6] Enter Test Step ts_ChangeSB1_ValueTag( )
| Assignment:[2] tcv_SB1_ValueTag := 3 Assignment:[2] sysInfoTypeSB1 := 3 Assignment:[2] tcv_SB1_ValueTagChanged := GcTRUE Attach:[3] Enter Test Step ts_ChangeMIB_ValueTag( )
| Attach:[3] Exit Test Step ts_ChangeMIB_ValueTag
Attach:[6] Exit Test Step ts_ChangeSB1_ValueTag
Attach:[7] Enter Test Step ts_Scheduling( 1 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:10.120 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[7] Exit Test Step ts_Scheduling
00:00:10.130 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[8] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 1 , routingInfo: [rB_Identity: -1 ]} Attach:[9] Enter Test Step ts_SendSIB6::lt_CompleteSIB( systemInformationBlockType6 )
| 00:00:10.130 - Primitive: RLC_TR_DATA_REQ 00:00:10.130 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[76] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[9] Exit Test Step ts_SendSIB6::lt_CompleteSIB
Attach:[10] Enter Test Step ts_Scheduling( 1 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:10.130 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[10] Exit Test Step ts_Scheduling
00:00:10.150 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[11] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 1 , routingInfo: [rB_Identity: -1 ]} 00:00:10.150 - Primitive: RLC_TR_DATA_REQ 00:00:10.150 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[12] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[13] Enter Test Step ts_Scheduling( 1 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:10.150 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[13] Exit Test Step ts_Scheduling
00:00:10.170 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[14] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 1 , routingInfo: [rB_Identity: -1 ]} 00:00:10.170 - Primitive: RLC_TR_DATA_REQ 00:00:10.170 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[15] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[16] Enter Test Step ts_Scheduling( 1 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:10.170 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[16] Exit Test Step ts_Scheduling
00:00:10.180 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[17] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 1 , routingInfo: [rB_Identity: -1 ]} 00:00:10.180 - Primitive: RLC_TR_DATA_REQ 00:00:10.180 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[18] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[12] Exit Test Step ts_SendSIB6
Attach:[13] Enter Test Step ts_SendSIB7( { modeSpecificInfo: [f ...
| (view Test Step parameters) 00:00:10.180 - Primitive: o_SIB_PER_Encoding Assignment:[1] tcv_Segs := (view Assignment) Assignment:[1] tcv_SIB7 := (view Assignment) Attach:[4] Enter Test Step ts_Scheduling( 1 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:10.180 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[4] Exit Test Step ts_Scheduling
00:00:10.200 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[5] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 1 , routingInfo: [rB_Identity: -1 ]} Attach:[6] Enter Test Step ts_SendSIB7::lt_CompleteSIB( systemInformationBlockType7 )
| 00:00:10.200 - Primitive: RLC_TR_DATA_REQ 00:00:10.200 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[13] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[6] Exit Test Step ts_SendSIB7::lt_CompleteSIB
Attach:[7] Enter Test Step ts_SendSIB7::lt_ConcatWithSIB3( { modeSpecificInfo: [f ...
| (view Test Step parameters) 00:00:10.200 - Primitive: o_SIB_PER_Encoding Assignment:[14] seg1 := '100000101000000010000001'B 00:00:10.200 - Primitive: o_SIB_PER_Encoding Assignment:[14] seg2 := (view Assignment) Attach:[17] Enter Test Step ts_Scheduling( 1 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:10.200 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[17] Exit Test Step ts_Scheduling
00:00:10.210 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[18] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 1 , routingInfo: [rB_Identity: -1 ]} 00:00:10.210 - Primitive: RLC_TR_DATA_REQ 00:00:10.210 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[19] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[7] Exit Test Step ts_SendSIB7::lt_ConcatWithSIB3
Attach:[8] Enter Test Step ts_SendSIB7::lt_ConcatWithSIB18( { modeSpecificInfo: [f ...
| (view Test Step parameters) 00:00:10.210 - Primitive: o_SIB_PER_Encoding Assignment:[20] seg2 := '100010000001000000000010000000001'B Attach:[23] Enter Test Step ts_Scheduling( 1 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:10.210 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[23] Exit Test Step ts_Scheduling
00:00:10.230 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[24] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 1 , routingInfo: [rB_Identity: -1 ]} 00:00:10.230 - Primitive: RLC_TR_DATA_REQ 00:00:10.230 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[25] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[8] Exit Test Step ts_SendSIB7::lt_ConcatWithSIB18
Attach:[9] Enter Test Step ts_SendSIB7::lt_ConcatWithSIB4( { modeSpecificInfo: [f ...
| (view Test Step parameters) 00:00:10.230 - Primitive: o_SIB_PER_Encoding Assignment:[26] seg2 := (view Assignment) Attach:[29] Enter Test Step ts_Scheduling( 1 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:10.230 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[29] Exit Test Step ts_Scheduling
00:00:10.240 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[30] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 1 , routingInfo: [rB_Identity: -1 ]} 00:00:10.240 - Primitive: RLC_TR_DATA_REQ 00:00:10.240 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[31] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[9] Exit Test Step ts_SendSIB7::lt_ConcatWithSIB4
Attach:[13] Exit Test Step ts_SendSIB7
Attach:[14] Enter Test Step ts_SendSIB11( { sib12indicator: GcTR ...
| (view Test Step parameters) 00:00:10.260 - Primitive: o_SIB_PER_Encoding Assignment:[1] tcv_Segs := (view Assignment) Assignment:[17] sysInfoType11 := 3 Assignment:[17] scheduling := (view Assignment) Attach:[18] Enter Test Step ts_ChangeSB1_ValueTag( )
| Attach:[18] Exit Test Step ts_ChangeSB1_ValueTag
Attach:[19] Enter Test Step ts_Scheduling( 1 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:10.340 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[19] Exit Test Step ts_Scheduling
00:00:10.350 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[20] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 1 , routingInfo: [rB_Identity: -1 ]} 00:00:10.350 - Primitive: RLC_TR_DATA_REQ 00:00:10.350 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[21] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[22] Enter Test Step ts_Scheduling( 1 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:10.350 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[22] Exit Test Step ts_Scheduling
00:00:10.370 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[23] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 1 , routingInfo: [rB_Identity: -1 ]} 00:00:10.370 - Primitive: RLC_TR_DATA_REQ 00:00:10.370 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[24] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[25] Enter Test Step ts_Scheduling( 1 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:10.370 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[25] Exit Test Step ts_Scheduling
00:00:10.380 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[26] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 1 , routingInfo: [rB_Identity: -1 ]} 00:00:10.380 - Primitive: RLC_TR_DATA_REQ 00:00:10.380 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[28] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[14] Exit Test Step ts_SendSIB11
Attach:[15] Enter Test Step ts_SendSIB12( { fach_MeasurementOcca ...
| (view Test Step parameters) 00:00:10.380 - Primitive: o_SIB_PER_Encoding Assignment:[1] tcv_Segs := (view Assignment) Assignment:[5] sysInfoType12 := 3 Assignment:[5] scheduling := { scheduling: { segCount: OMIT, sib_Pos: [rep64: 13 ], sib_PosOffsetInfo: OMIT} } Attach:[6] Enter Test Step ts_ChangeSB1_ValueTag( )
| Attach:[6] Exit Test Step ts_ChangeSB1_ValueTag
Attach:[7] Enter Test Step ts_Scheduling( 1 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:10.380 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[7] Exit Test Step ts_Scheduling
00:00:10.400 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[8] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 1 , routingInfo: [rB_Identity: -1 ]} Attach:[9] Enter Test Step ts_SendSIB12::lt_CompleteSIB( systemInformationBlockType12 )
| 00:00:10.400 - Primitive: RLC_TR_DATA_REQ 00:00:10.400 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[50] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[9] Exit Test Step ts_SendSIB12::lt_CompleteSIB
Attach:[10] Enter Test Step ts_Scheduling( 1 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:10.400 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[10] Exit Test Step ts_Scheduling
00:00:10.420 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[11] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 1 , routingInfo: [rB_Identity: -1 ]} 00:00:10.420 - Primitive: RLC_TR_DATA_REQ 00:00:10.420 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[12] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[13] Enter Test Step ts_Scheduling( 1 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:10.420 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[13] Exit Test Step ts_Scheduling
00:00:10.430 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[14] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 1 , routingInfo: [rB_Identity: -1 ]} 00:00:10.430 - Primitive: RLC_TR_DATA_REQ 00:00:10.430 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[15] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[15] Exit Test Step ts_SendSIB12
Attach:[16] Enter Test Step ts_SendSIB18( { idleModePLMNIdentiti ...
| (view Test Step parameters) Assignment:[1] tcv_SIB18 := (view Assignment) 00:00:10.430 - Primitive: o_SIB_PER_Encoding Assignment:[1] seg1 := '100010000001000000000010000000001'B 00:00:10.430 - Primitive: o_SIB_PER_Encoding Assignment:[1] seg2 := '100000101000000010000001'B Attach:[4] Enter Test Step ts_Scheduling( 1 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:10.430 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[4] Exit Test Step ts_Scheduling
00:00:10.450 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[5] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 1 , routingInfo: [rB_Identity: -1 ]} 00:00:10.450 - Primitive: RLC_TR_DATA_REQ 00:00:10.450 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[6] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Assignment:[7] sysInfoType18 := 3 Attach:[8] Enter Test Step ts_ChangeSB1_ValueTag( )
| Attach:[8] Exit Test Step ts_ChangeSB1_ValueTag
Attach:[16] Exit Test Step ts_SendSIB18
Attach:[17] Enter Test Step ts_SendSB1_DefSchedul( { sib_ReferenceList: [ ...
| (view Test Step parameters) 00:00:10.450 - Primitive: o_SIB_PER_Encoding Assignment:[1] tcv_Segs := (view Assignment) Attach:[3] Enter Test Step ts_Scheduling( 1 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:10.450 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[3] Exit Test Step ts_Scheduling
00:00:10.460 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[4] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 1 , routingInfo: [rB_Identity: -1 ]} Attach:[5] Enter Test Step ts_SendSB1_DefSchedul::lt_CompleteSIB( schedulingBlock1 )
| 00:00:10.460 - Primitive: RLC_TR_DATA_REQ 00:00:10.460 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[12] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[5] Exit Test Step ts_SendSB1_DefSchedul::lt_CompleteSIB
Attach:[6] Enter Test Step ts_ChangeSB1_ValueTag( )
| Attach:[6] Exit Test Step ts_ChangeSB1_ValueTag
Assignment:[7] scheduling := { scheduling: { segCount: OMIT, sib_Pos: [rep16: 1 ], sib_PosOffsetInfo: OMIT} } Assignment:[7] tcv_SB1_ValueTagChanged := GcFALSE Attach:[17] Exit Test Step ts_SendSB1_DefSchedul
Attach:[18] Enter Test Step ts_SendMIB( { mib_ValueTag: 2 , pl ...
| (view Test Step parameters) Attach:[1] Enter Test Step ts_SetTmpCellInfo( 1 )
| Assignment:[4] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Assignment:[2] mcc := [ 0 , 0 , 1 ] Assignment:[2] mnc := [ 0 , 1 ] 00:00:10.480 - Primitive: o_SIB_PER_Encoding Assignment:[3] tcv_Segs := (view Assignment) Attach:[6] Enter Test Step ts_Scheduling( 1 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:10.480 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[6] Exit Test Step ts_Scheduling
00:00:10.490 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[7] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 1 , routingInfo: [rB_Identity: -1 ]} Attach:[8] Enter Test Step ts_SendMIB::lt_CompleteSIB( masterInformationBlock )
| 00:00:10.490 - Primitive: RLC_TR_DATA_REQ 00:00:10.490 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[13] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[8] Exit Test Step ts_SendMIB::lt_CompleteSIB
Assignment:[9] tcv_MIB_ValueTagChanged := GcFALSE Attach:[18] Exit Test Step ts_SendMIB
Attach:[4] Exit Test Step ts_SendDefSysInfo
Attach:[5] Exit Test Step ts_GMM_Config_CellA_CellB
Attach:[6] Enter Test Step ts_IdleUpdated( 0 )
| Attach:[2] Enter Test Step ts_GMM_IdleUpdated( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[6] Enter Test Step ts_GMM_IdleUpdated::lt_IdleUpdated_NMO_II( 0 )
| Attach:[40] Enter Test Step ts_MMI_UE_SwitchOn( )
| 00:00:10.510 - Primitive: MMI_CmdReq Send event:[2] Ut ! MMI_CmdReq = PDU: { cmd: "Please switch on the UE" } 00:00:11.480 - Primitive: MMI_CmdCnf begin "ca_MMI_CmdCnf" of type MMI_CmdCnf (SEQUENCE) [UNIVERSAL 16] begin "result" of type BOOLEAN [UNIVERSAL 1] matching GcTRUE against GcTRUE end "result" of type BOOLEAN end "ca_MMI_CmdCnf" of type MMI_CmdCnf Receive event:[3] Ut ? MMI_CmdCnf = PDU: { result: GcTRUE , resultString: OMIT} Assignment:[4] tcv_UE_SwitchedOn := GcTRUE Attach:[40] Exit Test Step ts_MMI_UE_SwitchOn
Attach:[41] Enter Test Step ts_RRC_ConnEst( 0 )
| Attach:[1] Enter Test Step ts_SS_PrepareCellRRC_ConnEst( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[1] Exit Test Step ts_SS_PrepareCellRRC_ConnEst
Attach:[2] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[2] Exit Test Step ts_SetTmpCellInfo
Attach:[3] Enter Test Step ts_RRC_ConnEst::lt_RcvConnReq( 0 )
| 00:00:41.680 - Primitive: RLC_TR_DATA_IND: rrcConnectionRequest 00:00:41.680 - Primitive: RLC_TR_DATA_IND begin "car_RRC_ConnReq" of type RLC_TR_DATA_IND (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "tM_message" of type CHOICE [UNIVERSAL 31] begin "uL_CCCH_Message" of type UL_CCCH_Message (SEQUENCE) [UNIVERSAL 16] begin "message" of type UL_CCCH_MessageType (CHOICE) [UNIVERSAL 31] begin "rrcConnectionRequest" of type RRCConnectionRequest (SEQUENCE) [UNIVERSAL 16] begin "initialUE_Identity" of type InitialUE_Identity (CHOICE) [UNIVERSAL 31] begin InitialUE_Identity (CHOICE) [UNIVERSAL 31] end InitialUE_Identity begin InitialUE_Identity (CHOICE) [UNIVERSAL 31] end InitialUE_Identity begin InitialUE_Identity (CHOICE) [UNIVERSAL 31] begin "p_TMSI_and_RAI" of type P_TMSI_and_RAI_GSM_MAP (SEQUENCE) [UNIVERSAL 16] matching { p_TMSI: '00010010001101000101011001111000'B , rai: { lai: { plmn_Identity: { mcc: [ 0 , 0 , 1 ] , mnc: [ 0 , 1 ] } , lac: '0000000000000010'B } , rac: '00000101'B } } against ? end "p_TMSI_and_RAI" of type P_TMSI_and_RAI_GSM_MAP end InitialUE_Identity matching [p_TMSI_and_RAI: { p_TMSI: '00010010001101000101011001111000'B , rai: { lai: { plmn_Identity: { mcc: [ 0 , 0 , 1 ] , mnc: [ 0 , 1 ] } , lac: '0000000000000010'B } , rac: '00000101'B } } ] against ([imsi: ?], [tmsi_and_LAI: ?], [p_TMSI_and_RAI: ?], [imei: ?]) end "initialUE_Identity" of type InitialUE_Identity begin "establishmentCause" of type EstablishmentCause (ENUMERATED) [UNIVERSAL 10] matching registration against registration end "establishmentCause" of type EstablishmentCause begin "protocolErrorIndicator" of type ProtocolErrorIndicator (ENUMERATED) [UNIVERSAL 10] matching noError against noError end "protocolErrorIndicator" of type ProtocolErrorIndicator end "rrcConnectionRequest" of type RRCConnectionRequest end "message" of type UL_CCCH_MessageType end "uL_CCCH_Message" of type UL_CCCH_Message end "tM_message" of type CHOICE end "car_RRC_ConnReq" of type RLC_TR_DATA_IND Assignment:[7] tcv_InitialUE_Id := (view Assignment) Receive event:[7] TM ? RLC_TR_DATA_IND = PDU (view PDU) Attach:[3] Exit Test Step ts_RRC_ConnEst::lt_RcvConnReq
Attach:[4] Enter Test Step ts_RRC_ConnEst::lt_Send_ConnSetUp( 0 )
| 00:00:41.680 - Primitive: RLC_UM_DATA_REQ 00:00:41.700 - Primitive: RLC_UM_DATA_REQ: rrcConnectionSetup Send event:[31] UM ! RLC_UM_DATA_REQ = PDU (view PDU) Attach:[33] Enter Test Step ts_SetCellCfg( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Assignment:[2] cellConfig := cell_DCH_StandAloneSRB Attach:[3] Enter Test Step ts_SaveCellInfo( 0 )
| Assignment:[2] tcv_CellInfoA := (view Assignment) Attach:[3] Exit Test Step ts_SaveCellInfo
Attach:[33] Exit Test Step ts_SetCellCfg
Attach:[4] Exit Test Step ts_RRC_ConnEst::lt_Send_ConnSetUp
Attach:[5] Enter Test Step ts_RRC_ReceiveConnSetupCmpl( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
StartTimer:[3] t_WaitMS [13500] 13500 ms 00:00:42.180 - Primitive: RLC_AM_DATA_IND: rrcConnectionSetupComplete 00:00:42.180 - Primitive: RLC_AM_DATA_IND begin "car_RRC_ConnSetupCmpl" of type RLC_AM_DATA_IND (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "integrityResult" of type IntegrityResult (CHOICE) [UNIVERSAL 31] matching [integrityUsed: i_pass] against ? end "integrityResult" of type IntegrityResult begin "aM_message" of type CHOICE [UNIVERSAL 31] begin "uL_DCCH_Message" of type UL_DCCH_Message (SEQUENCE) [UNIVERSAL 16] begin "message" of type UL_DCCH_MessageType (CHOICE) [UNIVERSAL 31] begin "rrcConnectionSetupComplete" of type RRCConnectionSetupComplete (SEQUENCE) [UNIVERSAL 16] begin "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier (INTEGER) [UNIVERSAL 2] matching 0 against 0 end "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier begin "startList" of type STARTList (SEQUENCEOF) [UNIVERSAL 28] matching [ { cn_DomainIdentity: ps_domain, start_Value: '00000000000000000010'B } , { cn_DomainIdentity: cs_domain, start_Value: '00000000000000000010'B } ] against ? end "startList" of type STARTList begin "ue_RadioAccessCapability" of type UE_RadioAccessCapability (SEQUENCE) [UNIVERSAL 16] matching { accessStratumReleaseIndicator: r99, pdcp_Capability: { losslessSRNS_RelocationSupport: GcFALSE , supportForRfc2507: [notSupported: NULL]} , rlc_Capability: { totalRLC_AM_BufferSize: kb50, maximumRLC_WindowSize: mws2047, maximumAM_EntityNumber: am6} , transportChannelCapability: { dl_TransChCapability: { maxNoBitsReceived: b8960, maxConvCodeBitsReceived: b1280, turboDecodingSupport: [supported: b8960], maxSimultaneousTransChs: e8, maxSimultaneousCCTrCH_Count: 1 , maxReceivedTransportBlocks: tb32, maxNumberOfTFC: tfc128, maxNumberOfTF: tf64} , ul_TransChCapability: { maxNoBitsTransmitted: b3840, maxConvCodeBitsTransmitted: b1280, turboEncodingSupport: [supported: b3840], maxSimultaneousTransChs: e8, modeSpecificInfo: [fdd: NULL], maxTransmittedBlocks: tb32, maxNumberOfTFC: tfc64, maxNumberOfTF: tf32} } , rf_Capability: { fddRF_Capability: { ue_PowerClass: 4 , txRxFrequencySeparation: mhz190} , tddRF_Capability: OMIT} , physicalChannelCapability: { fddPhysChCapability: { downlinkPhysChCapability: { maxNoDPCH_PDSCH_Codes: 1 , maxNoPhysChBitsReceived: b9600, supportForSF_512: GcFALSE , supportOfPDSCH: GcFALSE , simultaneousSCCPCH_DPCH_Reception: [notSupported: NULL]} , uplinkPhysChCapability: { maxNoDPDCH_BitsTransmitted: b4800, supportOfPCPCH: GcFALSE } } , tddPhysChCapability: OMIT} , ue_MultiModeRAT_Capability: { multiRAT_CapabilityList: { supportOfGSM: GcFALSE , supportOfMulticarrier: GcFALSE } , multiModeCapability: fdd} , securityCapability: { cipheringAlgorithmCap: '0000000000000011'B , integrityProtectionAlgorithmCap: '0000000000000010'B } , ue_positioning_Capability: { standaloneLocMethodsSupported: GcFALSE , ue_BasedOTDOA_Supported: GcFALSE , networkAssistedGPS_Supported: noNetworkAssistedGPS, supportForUE_GPS_TimingOfCellFrames: GcFALSE , supportForIPDL: GcFALSE } , measurementCapability: { downlinkCompressedMode: { fdd_Measurements: GcTRUE , tdd_Measurements: OMIT, gsm_Measurements: { gsm900: GcTRUE , dcs1800: GcTRUE , gsm1900: GcTRUE } , multiCarrierMeasurements: GcFALSE } , uplinkCompressedMode: { fdd_Measurements: GcTRUE , tdd_Measurements: OMIT, gsm_Measurements: { gsm900: GcTRUE , dcs1800: GcTRUE , gsm1900: GcTRUE } , multiCarrierMeasurements: GcFALSE } } } against * end "ue_RadioAccessCapability" of type UE_RadioAccessCapability end "rrcConnectionSetupComplete" of type RRCConnectionSetupComplete end "message" of type UL_DCCH_MessageType end "uL_DCCH_Message" of type UL_DCCH_Message end "aM_message" of type CHOICE end "car_RRC_ConnSetupCmpl" of type RLC_AM_DATA_IND Assignment:TSP1: [5] tcv_StartList := (view Assignment) Assignment:TSP1: [5] cipheringAlgorithmCapability := '0000000000000011'B CancelTimer:TSP1: [5] t_WaitMS [13500] 13500 ms Receive event:TSP1: [5] AM ? RLC_AM_DATA_IND = PDU (view PDU) Preliminary verdict:TSP1: [5] (PASS) Attach:[6] Enter Test Step ts_RRC_ReceiveConnSetupCmpl::lt_GetHFN( 0 )
| Assignment:[13] tcv_Count := 2 Attach:[17] Enter Test Step ts_RRC_ReceiveConnSetupCmpl::lt_FirstValue( 0 )
| Assignment:[23] start_PS := '00000000000000000010'B Attach:[17] Exit Test Step ts_RRC_ReceiveConnSetupCmpl::lt_FirstValue
Attach:[18] Enter Test Step ts_RRC_ReceiveConnSetupCmpl::lt_SecondValue( 0 )
| Assignment:[26] start_CS := '00000000000000000010'B Attach:[18] Exit Test Step ts_RRC_ReceiveConnSetupCmpl::lt_SecondValue
Attach:[6] Exit Test Step ts_RRC_ReceiveConnSetupCmpl::lt_GetHFN
Attach:[5] Exit Test Step ts_RRC_ReceiveConnSetupCmpl
Attach:[41] Exit Test Step ts_RRC_ConnEst
00:00:42.190 - Primitive: RLC_AM_DATA_IND: initialDirectTransfer 00:00:42.190 - Primitive: RRC_DATA_IND: mm:locationUpdatingRequest begin "car_InitDirectTransfer" of type RRC_DataInd (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "rB_Id" of type SS_RB_Identity (INTEGER) [UNIVERSAL 2] matching 3 against 3 end "rB_Id" of type SS_RB_Identity begin "cN_Domain" of type SS_CN_DomainIdentity (INTEGER) [UNIVERSAL 2] matching 0 against 0 end "cN_Domain" of type SS_CN_DomainIdentity begin "start" of type START_Value (BITSTRING) [UNIVERSAL 3] matching '00000000000000000010'B against ? end "start" of type START_Value begin "msg" of type LOCATIONUPDATINGREQUEST (SEQUENCE) [UNIVERSAL 16] begin "skipIndicator" of type SkipIndicator (BITSTRING) [UNIVERSAL 3] matching '0000'B against '0000'B end "skipIndicator" of type SkipIndicator begin "mMProtocolDiscriminator" of type ProtocolDiscriminator (BITSTRING) [UNIVERSAL 3] matching '0101'B against '0101'B end "mMProtocolDiscriminator" of type ProtocolDiscriminator begin "msgType" of type MsgType (BITSTRING) [UNIVERSAL 3] matching '00001000'B against '??001000'B end "msgType" of type MsgType begin "ciphKeySeqNum" of type CiphKeySeqNum (SEQUENCE) [UNIVERSAL 16] begin "spare1" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against '0'B end "spare1" of type B1 begin "keySeq" of type KeySeq (BITSTRING) [UNIVERSAL 3] matching '111'B against ? end "keySeq" of type KeySeq end "ciphKeySeqNum" of type CiphKeySeqNum begin "locUpdType" of type LocUpdType (SEQUENCE) [UNIVERSAL 16] begin "fOR" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against ? end "fOR" of type B1 begin "spare1" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against '0'B end "spare1" of type B1 begin "lUT" of type B2 (BITSTRING) [UNIVERSAL 3] matching '00'B against ? end "lUT" of type B2 end "locUpdType" of type LocUpdType begin "locAreaId" of type LocAreaId_v (SEQUENCE) [UNIVERSAL 16] begin "plmn" of type OCTETSTRING [UNIVERSAL 4] matching '00F110'O against ? end "plmn" of type OCTETSTRING begin "lac" of type OCTETSTRING [UNIVERSAL 4] matching 'FFFE'O against ? end "lac" of type OCTETSTRING end "locAreaId" of type LocAreaId_v begin "mSClsmk1" of type MS_Clsmk1 (SEQUENCE) [UNIVERSAL 16] begin "spare1" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against '0'B end "spare1" of type B1 begin "revLvl" of type B2 (BITSTRING) [UNIVERSAL 3] matching '10'B against ? end "revLvl" of type B2 begin "eSIND" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against ? end "eSIND" of type B1 begin "a5_1" of type B1 (BITSTRING) [UNIVERSAL 3] matching '1'B against ? end "a5_1" of type B1 begin "rFPwrCap" of type B3 (BITSTRING) [UNIVERSAL 3] matching '111'B against ? end "rFPwrCap" of type B3 end "mSClsmk1" of type MS_Clsmk1 begin "mobileId" of type MS_Identity_lv (SEQUENCE) [UNIVERSAL 16] begin "iel" of type Length (OCTETSTRING) [UNIVERSAL 4] matching '08'O against ? end "iel" of type Length begin "iDigit1" of type B4 (BITSTRING) [UNIVERSAL 3] matching '0000'B against ? end "iDigit1" of type B4 begin "oddEvenInd" of type B1 (BITSTRING) [UNIVERSAL 3] matching '1'B against ? end "oddEvenInd" of type B1 begin "typeOfId" of type B3 (BITSTRING) [UNIVERSAL 3] matching '001'B against ? end "typeOfId" of type B3 begin "otherDigits" of type OCTETSTRING [UNIVERSAL 4] matching '10100000003033'O against ? end "otherDigits" of type OCTETSTRING end "mobileId" of type MS_Identity_lv begin "mSClsmk2" of type MS_Clsmk2 (SEQUENCE) [UNIVERSAL 16] begin "iei" of type IEI8 (BITSTRING) [UNIVERSAL 3] matching '00110011'B against '00110011'B end "iei" of type IEI8 begin "iel" of type Length (OCTETSTRING) [UNIVERSAL 4] matching '03'O against '03'O end "iel" of type Length begin "spare1_1" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against '0'B end "spare1_1" of type B1 begin "revLvl" of type B2 (BITSTRING) [UNIVERSAL 3] matching '10'B against ? end "revLvl" of type B2 begin "eSIND" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against ? end "eSIND" of type B1 begin "a5_1" of type B1 (BITSTRING) [UNIVERSAL 3] matching '1'B against ? end "a5_1" of type B1 begin "rFPwrCap" of type B3 (BITSTRING) [UNIVERSAL 3] matching '111'B against ? end "rFPwrCap" of type B3 begin "spare1_2" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against '0'B end "spare1_2" of type B1 begin "pSCap" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against ? end "pSCap" of type B1 begin "sSSI" of type B2 (BITSTRING) [UNIVERSAL 3] matching '01'B against ? end "sSSI" of type B2 begin "sMCap" of type B1 (BITSTRING) [UNIVERSAL 3] matching '1'B against ? end "sMCap" of type B1 begin "vBS" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against ? end "vBS" of type B1 begin "vGCS" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against ? end "vGCS" of type B1 begin "fC" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against ? end "fC" of type B1 begin "cM3" of type B1 (BITSTRING) [UNIVERSAL 3] matching '1'B against ? end "cM3" of type B1 begin "spare1_3" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against '0'B end "spare1_3" of type B1 begin "lCSVA" of type B1 (BITSTRING) [UNIVERSAL 3] matching '1'B against ? end "lCSVA" of type B1 begin "uCS2" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against ? end "uCS2" of type B1 begin "soLSA" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against ? end "soLSA" of type B1 begin "cMSP" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against ? end "cMSP" of type B1 begin "a5_3" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against ? end "a5_3" of type B1 begin "a5_2" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against ? end "a5_2" of type B1 end "mSClsmk2" of type MS_Clsmk2 end "msg" of type LOCATIONUPDATINGREQUEST end "car_InitDirectTransfer" of type RRC_DataInd Assignment:[42] tcv_Start := '00000000000000000010'B Receive event:[42] Dc ? RRC_DataInd = PDU (view PDU) Assignment:[43] tcv_GMM_AttachExpect := GcTRUE Assignment:[43] tcv_GMM_AttachRec := GcFALSE Attach:[44] Enter Test Step ts_SS_SecurityDownloadStart( cs_domain )
| Assignment:[2] start_CS := '00000000000000000010'B Attach:[44] Exit Test Step ts_SS_SecurityDownloadStart
Attach:[45] Enter Test Step ts_MM_Authentication( 0 )
| Attach:[1] Enter Test Step ts_MM_AuthenticationInit( )
| Attach:[1] Enter Test Step ts_MM_AuthenticationInit::lt_IncrementCiphKeySeqNum( )
| Assignment:[18] tcv_CS_KeySeq := '000'B Attach:[1] Exit Test Step ts_MM_AuthenticationInit::lt_IncrementCiphKeySeqNum
Attach:[2] Enter Test Step ts_MM_AuthenticationInit::lt_AuthCalcAUTN( )
| Assignment:[19] tcv_AuthXDOUT := (view Assignment) Assignment:[20] tcv_AuthCDOUT := '0000000000000000000000000000000000000000000000000000000000000000'B Assignment:[21] tcv_AuthXDOUT_Half := '0101010101000100011101110110011000010001000000000011001100100010'B Assignment:[22] tcv_AuthAK := '011001100001000100000000001100110010001011011101'B Assignment:[23] tcv_AuthAUTN_1 := '011001100001000100000000001100110010001011011101'B Assignment:[24] tcv_AuthMAC := '0101010101000100011101110110011000010001000000000011001100100010'B Assignment:[25] tcv_AuthAUTN_2 := (view Assignment) Assignment:[26] tcv_AuthAUTN := (view Assignment) Attach:[2] Exit Test Step ts_MM_AuthenticationInit::lt_AuthCalcAUTN
Attach:[3] Enter Test Step ts_MM_AuthenticationInit::lt_AuthCalcUMTS_Others( )
| Assignment:[27] tcv_AuthIK := (view Assignment) Assignment:[28] tcv_AuthCK := (view Assignment) Assignment:[29] tcv_AuthXRES := (view Assignment) Attach:[3] Exit Test Step ts_MM_AuthenticationInit::lt_AuthCalcUMTS_Others
Attach:[4] Enter Test Step ts_MM_AuthenticationInit::lt_AuthCalcKcGSM( )
| Assignment:[30] tcv_AuthCK_1 := '0100010001110111011001100001000100000000001100110010001011011101'B Assignment:[31] tcv_AuthCK_2 := '1100110011111111111011101001100110001000101110111010101001010101'B Assignment:[32] tcv_AuthIK_1 := '0111011101100110000100010000000000110011001000101101110111001100'B Assignment:[33] tcv_AuthIK_2 := '1111111111101110100110011000100010111011101010100101010101000100'B Assignment:[34] tcv_AuthCK_XOR := '1000100010001000100010001000100010001000100010001000100010001000'B Assignment:[35] tcv_AuthIK_XOR := '1000100010001000100010001000100010001000100010001000100010001000'B Assignment:[36] tcv_AuthKcGSM := '0000000000000000000000000000000000000000000000000000000000000000'B Attach:[4] Exit Test Step ts_MM_AuthenticationInit::lt_AuthCalcKcGSM
Attach:[1] Exit Test Step ts_MM_AuthenticationInit
00:00:42.230 - Primitive: RRC_DATA_REQ: mm:authenticationRequest 00:00:42.230 - Primitive: RLC_AM_DATA_REQ:downlinkDirectTransfer Send event:[2] Dc ! RRC_DataReq = PDU (view PDU) 00:00:42.220 - Primitive: RLC_AM_DATA_IND: initialDirectTransfer 00:00:42.220 - Primitive: RRC_DATA_IND: gmm:attachRequest begin "car_UplinkDirectTransfer" of type RRC_DataInd (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "rB_Id" of type SS_RB_Identity (INTEGER) [UNIVERSAL 2] matching 3 against 3 end "rB_Id" of type SS_RB_Identity begin "cN_Domain" of type SS_CN_DomainIdentity (INTEGER) [UNIVERSAL 2] matching 1 against 0 end "cN_Domain" of type SS_CN_DomainIdentity end "car_UplinkDirectTransfer" of type RRC_DataInd Match failed [#1] : (view details)
Expected | RRC_DataInd
Received | RRC_DataInd
begin "car_UplinkDirectTransfer" of type RRC_DataInd (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "rB_Id" of type SS_RB_Identity (INTEGER) [UNIVERSAL 2] matching 3 against 3 end "rB_Id" of type SS_RB_Identity begin "cN_Domain" of type SS_CN_DomainIdentity (INTEGER) [UNIVERSAL 2] matching 1 against 0 end "cN_Domain" of type SS_CN_DomainIdentity end "car_UplinkDirectTransfer" of type RRC_DataInd Match failed [#2] : (view details)
Expected | RRC_DataInd
Received | RRC_DataInd
begin "car_UplinkDirectTransfer" of type RRC_DataInd (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "rB_Id" of type SS_RB_Identity (INTEGER) [UNIVERSAL 2] matching 3 against 3 end "rB_Id" of type SS_RB_Identity begin "cN_Domain" of type SS_CN_DomainIdentity (INTEGER) [UNIVERSAL 2] matching 1 against 0 end "cN_Domain" of type SS_CN_DomainIdentity end "car_UplinkDirectTransfer" of type RRC_DataInd Match failed [#3] : (view details)
Expected | RRC_DataInd
Received | RRC_DataInd
begin "car_PS_InitDirectTransfer" of type RRC_DataInd (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "rB_Id" of type SS_RB_Identity (INTEGER) [UNIVERSAL 2] matching 3 against 3 end "rB_Id" of type SS_RB_Identity begin "cN_Domain" of type SS_CN_DomainIdentity (INTEGER) [UNIVERSAL 2] matching 1 against 1 end "cN_Domain" of type SS_CN_DomainIdentity begin "start" of type START_Value (BITSTRING) [UNIVERSAL 3] matching '00000000000000000010'B against ? end "start" of type START_Value begin "msg" of type ATTACHREQUEST (SEQUENCE) [UNIVERSAL 16] begin "skipIndicator" of type SkipIndicator (BITSTRING) [UNIVERSAL 3] matching '0000'B against '0000'B end "skipIndicator" of type SkipIndicator begin "gMMProtocolDiscriminator" of type ProtocolDiscriminator (BITSTRING) [UNIVERSAL 3] matching '1000'B against '1000'B end "gMMProtocolDiscriminator" of type ProtocolDiscriminator begin "msgType" of type MsgType (BITSTRING) [UNIVERSAL 3] matching '00000001'B against '00000001'B end "msgType" of type MsgType begin "msNetworkCap" of type MS_NetworkCap_lv (SEQUENCE) [UNIVERSAL 16] matching { iel: '02'O , value: 'E540'O } against ? end "msNetworkCap" of type MS_NetworkCap_lv begin "gprsCiphKeySeqNo" of type CiphKeySeqNum (SEQUENCE) [UNIVERSAL 16] begin "spare1" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against '0'B end "spare1" of type B1 begin "keySeq" of type KeySeq (BITSTRING) [UNIVERSAL 3] matching '000'B against ? end "keySeq" of type KeySeq end "gprsCiphKeySeqNo" of type CiphKeySeqNum begin "attachType" of type AttachType (SEQUENCE) [UNIVERSAL 16] begin "for" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against ? end "for" of type B1 begin "type" of type B3 (BITSTRING) [UNIVERSAL 3] matching '001'B against ? end "type" of type B3 end "attachType" of type AttachType begin "drxParameter" of type DRXparamter (SEQUENCE) [UNIVERSAL 16] matching { splitPGcycleCode: '00000111'B , cnDRXcoef: '0000'B , splitOnCCCH: '0'B , nonDRXtimer: '100'B } against ? end "drxParameter" of type DRXparamter begin "ptmsiORimsi" of type MS_Identity_lv (SEQUENCE) [UNIVERSAL 16] begin "iel" of type Length (OCTETSTRING) [UNIVERSAL 4] matching '05'O against ? end "iel" of type Length begin "iDigit1" of type B4 (BITSTRING) [UNIVERSAL 3] matching '1111'B against ? end "iDigit1" of type B4 begin "oddEvenInd" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against ? end "oddEvenInd" of type B1 begin "typeOfId" of type B3 (BITSTRING) [UNIVERSAL 3] matching '100'B against ? end "typeOfId" of type B3 begin "otherDigits" of type OCTETSTRING [UNIVERSAL 4] matching '12345678'O against ? end "otherDigits" of type OCTETSTRING end "ptmsiORimsi" of type MS_Identity_lv begin "oldRAI" of type RAI_v (SEQUENCE) [UNIVERSAL 16] begin "plmn" of type OCTETSTRING [UNIVERSAL 4] matching '00F110'O against ? end "plmn" of type OCTETSTRING begin "lac" of type OCTETSTRING [UNIVERSAL 4] matching '0002'O against ? end "lac" of type OCTETSTRING begin "rac" of type OCTETSTRING [UNIVERSAL 4] matching '05'O against ? end "rac" of type OCTETSTRING end "oldRAI" of type RAI_v begin "msRadioAccessCap" of type MSRadioAccessCap_lv (SEQUENCE) [UNIVERSAL 16] matching { iel: '0B'O , value: '15F38233542A332644A198'O } against ? end "msRadioAccessCap" of type MSRadioAccessCap_lv begin "readyTimer" of type GPRS_Timer (SEQUENCE) [UNIVERSAL 16] begin "iei" of type IEI8 (BITSTRING) [UNIVERSAL 3] matching '00010111'B against '00010111'B end "iei" of type IEI8 begin "unit" of type B3 (BITSTRING) [UNIVERSAL 3] matching '000'B against ? end "unit" of type B3 begin "value" of type B5 (BITSTRING) [UNIVERSAL 3] matching '10110'B against ? end "value" of type B5 end "readyTimer" of type GPRS_Timer end "msg" of type ATTACHREQUEST end "car_PS_InitDirectTransfer" of type RRC_DataInd begin "car_PS_InitDirectTransfer" of type RRC_DataInd (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "rB_Id" of type SS_RB_Identity (INTEGER) [UNIVERSAL 2] matching 3 against 3 end "rB_Id" of type SS_RB_Identity begin "cN_Domain" of type SS_CN_DomainIdentity (INTEGER) [UNIVERSAL 2] matching 1 against 1 end "cN_Domain" of type SS_CN_DomainIdentity begin "start" of type START_Value (BITSTRING) [UNIVERSAL 3] matching '00000000000000000010'B against ? end "start" of type START_Value begin "msg" of type ATTACHREQUEST (SEQUENCE) [UNIVERSAL 16] begin "skipIndicator" of type SkipIndicator (BITSTRING) [UNIVERSAL 3] matching '0000'B against '0000'B end "skipIndicator" of type SkipIndicator begin "gMMProtocolDiscriminator" of type ProtocolDiscriminator (BITSTRING) [UNIVERSAL 3] matching '1000'B against '1000'B end "gMMProtocolDiscriminator" of type ProtocolDiscriminator begin "msgType" of type MsgType (BITSTRING) [UNIVERSAL 3] matching '00000001'B against '00000001'B end "msgType" of type MsgType begin "msNetworkCap" of type MS_NetworkCap_lv (SEQUENCE) [UNIVERSAL 16] matching { iel: '02'O , value: 'E540'O } against ? end "msNetworkCap" of type MS_NetworkCap_lv begin "gprsCiphKeySeqNo" of type CiphKeySeqNum (SEQUENCE) [UNIVERSAL 16] begin "spare1" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against '0'B end "spare1" of type B1 begin "keySeq" of type KeySeq (BITSTRING) [UNIVERSAL 3] matching '000'B against ? end "keySeq" of type KeySeq end "gprsCiphKeySeqNo" of type CiphKeySeqNum begin "attachType" of type AttachType (SEQUENCE) [UNIVERSAL 16] begin "for" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against ? end "for" of type B1 begin "type" of type B3 (BITSTRING) [UNIVERSAL 3] matching '001'B against ? end "type" of type B3 end "attachType" of type AttachType begin "drxParameter" of type DRXparamter (SEQUENCE) [UNIVERSAL 16] matching { splitPGcycleCode: '00000111'B , cnDRXcoef: '0000'B , splitOnCCCH: '0'B , nonDRXtimer: '100'B } against ? end "drxParameter" of type DRXparamter begin "ptmsiORimsi" of type MS_Identity_lv (SEQUENCE) [UNIVERSAL 16] begin "iel" of type Length (OCTETSTRING) [UNIVERSAL 4] matching '05'O against ? end "iel" of type Length begin "iDigit1" of type B4 (BITSTRING) [UNIVERSAL 3] matching '1111'B against ? end "iDigit1" of type B4 begin "oddEvenInd" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against ? end "oddEvenInd" of type B1 begin "typeOfId" of type B3 (BITSTRING) [UNIVERSAL 3] matching '100'B against ? end "typeOfId" of type B3 begin "otherDigits" of type OCTETSTRING [UNIVERSAL 4] matching '12345678'O against ? end "otherDigits" of type OCTETSTRING end "ptmsiORimsi" of type MS_Identity_lv begin "oldRAI" of type RAI_v (SEQUENCE) [UNIVERSAL 16] begin "plmn" of type OCTETSTRING [UNIVERSAL 4] matching '00F110'O against ? end "plmn" of type OCTETSTRING begin "lac" of type OCTETSTRING [UNIVERSAL 4] matching '0002'O against ? end "lac" of type OCTETSTRING begin "rac" of type OCTETSTRING [UNIVERSAL 4] matching '05'O against ? end "rac" of type OCTETSTRING end "oldRAI" of type RAI_v begin "msRadioAccessCap" of type MSRadioAccessCap_lv (SEQUENCE) [UNIVERSAL 16] matching { iel: '0B'O , value: '15F38233542A332644A198'O } against ? end "msRadioAccessCap" of type MSRadioAccessCap_lv begin "readyTimer" of type GPRS_Timer (SEQUENCE) [UNIVERSAL 16] begin "iei" of type IEI8 (BITSTRING) [UNIVERSAL 3] matching '00010111'B against '00010111'B end "iei" of type IEI8 begin "unit" of type B3 (BITSTRING) [UNIVERSAL 3] matching '000'B against ? end "unit" of type B3 begin "value" of type B5 (BITSTRING) [UNIVERSAL 3] matching '10110'B against ? end "value" of type B5 end "readyTimer" of type GPRS_Timer end "msg" of type ATTACHREQUEST end "car_PS_InitDirectTransfer" of type RRC_DataInd Assignment:[19] tcv_TmpAttachReqPDU (view PDU) Assignment:[19] tcv_TmpB3 := '001'B Assignment:[19] start_PS := '00000000000000000010'B Assignment:[19] tcv_GMM_AttachRec := GcTRUE Receive event:[19] Dc ? RRC_DataInd = PDU (view PDU) 00:00:42.670 - Primitive: RLC_AM_DATA_IND: uplinkDirectTransfer 00:00:42.670 - Primitive: RRC_DATA_IND: mm:authenticationResponse begin "car_UplinkDirectTransfer" of type RRC_DataInd (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "rB_Id" of type SS_RB_Identity (INTEGER) [UNIVERSAL 2] matching 3 against 3 end "rB_Id" of type SS_RB_Identity begin "cN_Domain" of type SS_CN_DomainIdentity (INTEGER) [UNIVERSAL 2] matching 0 against 0 end "cN_Domain" of type SS_CN_DomainIdentity begin "msg" of type AUTHENTICATIONRESPONSE (SEQUENCE) [UNIVERSAL 16] begin "skipIndicator" of type SkipIndicator (BITSTRING) [UNIVERSAL 3] matching '0000'B against '0000'B end "skipIndicator" of type SkipIndicator begin "mMProtocolDiscriminator" of type ProtocolDiscriminator (BITSTRING) [UNIVERSAL 3] matching '0101'B against '0101'B end "mMProtocolDiscriminator" of type ProtocolDiscriminator begin "msgType" of type MsgType (BITSTRING) [UNIVERSAL 3] matching '01010100'B against '??010100'B end "msgType" of type MsgType begin "authRsp" of type AuthRsp (BITSTRING) [UNIVERSAL 3] matching '01010101010001000111011101100110'B against ? end "authRsp" of type AuthRsp begin "authRspExt" of type AuthRspExt (SEQUENCE) [UNIVERSAL 16] begin "iei" of type IEI8 (BITSTRING) [UNIVERSAL 3] matching '00100001'B against '00100001'B end "iei" of type IEI8 begin "iel" of type Length (OCTETSTRING) [UNIVERSAL 4] matching '04'O against ? end "iel" of type Length begin "rES" of type BITSTRING [UNIVERSAL 3] matching '00010001000000000011001100100010'B against ? end "rES" of type BITSTRING end "authRspExt" of type AuthRspExt end "msg" of type AUTHENTICATIONRESPONSE end "car_UplinkDirectTransfer" of type RRC_DataInd Assignment:[3] tcv_AuthRspPDU (view PDU) Assignment:[3] tcv_AuthRsp := '01010101010001000111011101100110'B Assignment:[3] tcv_AuthRspExt := { iei: '00100001'B , iel: '04'O , rES: '00010001000000000011001100100010'B } Receive event:[3] Dc ? RRC_DataInd = PDU (view PDU) Assignment:[4] tcv_Res := GcTRUE Attach:[45] Exit Test Step ts_MM_Authentication
Attach:[46] Enter Test Step ts_RRC_Security( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[2] Enter Test Step ts_RRC_Security::lt_RRC_InitVariables( 0 )
| Attach:[53] Enter Test Step ts_RRC_Security::lt_InitCipherMode( 0 )
| Assignment:[82] cs_cipheringStarted := GcFALSE Assignment:[82] ps_cipheringStarted := GcFALSE Assignment:[84] cipheringAlgorithmCapability := '0000000000000011'B Attach:[53] Exit Test Step ts_RRC_Security::lt_InitCipherMode
Attach:[54] Enter Test Step ts_RRC_Security::lt_InitIntegrity( 0 )
| Assignment:[87] recentSecureDomain := cs_domain Assignment:[92] dL_Integrity := (view Assignment) Assignment:[92] integrityStarted := GcTRUE Assignment:[92] dl_IntegrityCheckInfo := (view Assignment) Assignment:[92] tcv_Int_ModifyFlag := GcFALSE Attach:[54] Exit Test Step ts_RRC_Security::lt_InitIntegrity
Attach:[55] Enter Test Step ts_InitSystemSpecificCap( )
| Assignment:[11] tcv_UE_SystemSpecificCap := 0 Attach:[55] Exit Test Step ts_InitSystemSpecificCap
Attach:[56] Enter Test Step ts_SaveCellInfo( 0 )
| Assignment:[2] tcv_CellInfoA := (view Assignment) Attach:[56] Exit Test Step ts_SaveCellInfo
Assignment:[58] tcv_HFN := '00000000000000000000'B Assignment:[60] start_CS := '00000000000000000000'B Attach:[2] Exit Test Step ts_RRC_Security::lt_RRC_InitVariables
Attach:[3] Enter Test Step ts_SS_DownloadSecurityKey( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[15] Enter Test Step ts_SS_DownloadSecurityKey::lt_DownloadKeyCRLC( '00000000000000000000'B )
| 00:00:42.680 - Primitive: CRLC_SecurityMode_Config_REQ 00:00:42.680 - Primitive: CRLC_SecurityMode_Config_REQ Send event:[21] CRLC ! CRLC_SecurityMode_Config_REQ = PDU (view PDU) 00:00:42.700 - Primitive: CRLC_SecurityMode_Config_CNF begin "ca_CRLC_SecurityModeCfgCnf" of type CRLC_SecurityMode_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER end "ca_CRLC_SecurityModeCfgCnf" of type CRLC_SecurityMode_Config_CNF Receive event:[22] CRLC ? CRLC_SecurityMode_Config_CNF = PDU: { cellId: -1 } Attach:[15] Exit Test Step ts_SS_DownloadSecurityKey::lt_DownloadKeyCRLC
Attach:[3] Exit Test Step ts_SS_DownloadSecurityKey
Attach:[4] Enter Test Step ts_RRC_Security::lt_ActivateSecurity_DL_SS( 0 )
| Attach:[14] Enter Test Step ts_RRC_Security::lt_InitialiseRRC_MSN( 0 )
| Attach:[25] Enter Test Step ts_SetDL_RRC_MessageSN( 0 )
| 00:00:42.700 - Primitive: CRLC_SetRRC_MessageSN_REQ Send event:[1] CRLC ! CRLC_SetRRC_MessageSN_REQ = PDU (view PDU) 00:00:42.710 - Primitive: CRLC_SetRRC_MessageSN_CNF begin "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF Receive event:[2] CRLC ? CRLC_SetRRC_MessageSN_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: 0 ]} 00:00:42.710 - Primitive: CRLC_SetRRC_MessageSN_REQ Send event:[3] CRLC ! CRLC_SetRRC_MessageSN_REQ = PDU (view PDU) 00:00:42.730 - Primitive: CRLC_SetRRC_MessageSN_CNF begin "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF Receive event:[4] CRLC ? CRLC_SetRRC_MessageSN_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 1 ]} 00:00:42.730 - Primitive: CRLC_SetRRC_MessageSN_REQ Send event:[5] CRLC ! CRLC_SetRRC_MessageSN_REQ = PDU (view PDU) 00:00:42.740 - Primitive: CRLC_SetRRC_MessageSN_CNF begin "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF Receive event:[6] CRLC ? CRLC_SetRRC_MessageSN_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 2 ]} 00:00:42.740 - Primitive: CRLC_SetRRC_MessageSN_REQ Send event:[7] CRLC ! CRLC_SetRRC_MessageSN_REQ = PDU (view PDU) 00:00:42.760 - Primitive: CRLC_SetRRC_MessageSN_CNF begin "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF Receive event:[8] CRLC ? CRLC_SetRRC_MessageSN_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 3 ]} 00:00:42.760 - Primitive: CRLC_SetRRC_MessageSN_REQ Send event:[9] CRLC ! CRLC_SetRRC_MessageSN_REQ = PDU (view PDU) 00:00:42.780 - Primitive: CRLC_SetRRC_MessageSN_CNF begin "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF Receive event:[10] CRLC ? CRLC_SetRRC_MessageSN_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 4 ]} Attach:[25] Exit Test Step ts_SetDL_RRC_MessageSN
Attach:[14] Exit Test Step ts_RRC_Security::lt_InitialiseRRC_MSN
Attach:[15] Enter Test Step ts_CRLC_DL_Integrity( { integrityProtectionM ...
| (view Test Step parameters) 00:00:42.780 - Primitive: CRLC_Integrity_Activate_REQ 00:00:42.780 - Primitive: CRLC_Integrity_Activate_REQ Send event:[1] CRLC ! CRLC_Integrity_Activate_REQ = PDU (view PDU) 00:00:42.790 - Primitive: CRLC_Integrity_Activate_CNF begin "ca_CRLC_IntegrityActivateCnf" of type CRLC_Integrity_Activate_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER end "ca_CRLC_IntegrityActivateCnf" of type CRLC_Integrity_Activate_CNF Receive event:[2] CRLC ? CRLC_Integrity_Activate_CNF = PDU: { cellId: -1 } Attach:[15] Exit Test Step ts_CRLC_DL_Integrity
Attach:[4] Exit Test Step ts_RRC_Security::lt_ActivateSecurity_DL_SS
Attach:[5] Enter Test Step ts_RRC_Security::lt_RB2_UL_IntegrityActivate( 0 )
| Attach:[13] Enter Test Step ts_RB2_UL_IntegrityActivate( 0 )
| 00:00:42.790 - Primitive: CRLC_Integrity_Activate_REQ 00:00:42.790 - Primitive: CRLC_Integrity_Activate_REQ Send event:[1] CRLC ! CRLC_Integrity_Activate_REQ = PDU (view PDU) 00:00:42.810 - Primitive: CRLC_Integrity_Activate_CNF begin "ca_CRLC_IntegrityActivateCnf" of type CRLC_Integrity_Activate_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER end "ca_CRLC_IntegrityActivateCnf" of type CRLC_Integrity_Activate_CNF Receive event:[2] CRLC ? CRLC_Integrity_Activate_CNF = PDU: { cellId: -1 } Attach:[13] Exit Test Step ts_RB2_UL_IntegrityActivate
Attach:[5] Exit Test Step ts_RRC_Security::lt_RB2_UL_IntegrityActivate
Attach:[6] Enter Test Step ts_RRC_Security::lt_StartSecurity_UE( 0 )
| Attach:[27] Enter Test Step ts_RRC_Security::lt_SendSecurityModeCommand( 0 )
| 00:00:42.810 - Primitive: RLC_AM_DATA_REQ 00:00:42.810 - Primitive: RLC_AM_DATA_REQ: securityModeCommand Send event:[52] AM ! RLC_AM_DATA_REQ = PDU (view PDU) Attach:[27] Exit Test Step ts_RRC_Security::lt_SendSecurityModeCommand
00:00:43.070 - Primitive: RLC_AM_DATA_IND: securityModeComplete 00:00:43.070 - Primitive: RLC_AM_DATA_IND begin "car_RRC_SecModeCmpl" of type RLC_AM_DATA_IND (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "integrityResult" of type IntegrityResult (CHOICE) [UNIVERSAL 31] matching [integrityUsed: i_pass] against * end "integrityResult" of type IntegrityResult begin "aM_message" of type CHOICE [UNIVERSAL 31] begin "uL_DCCH_Message" of type UL_DCCH_Message (SEQUENCE) [UNIVERSAL 16] begin "integrityCheckInfo" of type IntegrityCheckInfo (SEQUENCE) [UNIVERSAL 16] matching { messageAuthenticationCode: '10001011001000110111110011100010'B , rrc_MessageSequenceNumber: 1 } against * end "integrityCheckInfo" of type IntegrityCheckInfo begin "message" of type UL_DCCH_MessageType (CHOICE) [UNIVERSAL 31] begin "securityModeComplete" of type SecurityModeComplete (SEQUENCE) [UNIVERSAL 16] begin "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier (INTEGER) [UNIVERSAL 2] matching 0 against 0 end "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier begin "ul_IntegProtActivationInfo" of type IntegrityProtActivationInfo (SEQUENCE) [UNIVERSAL 16] matching { rrc_MessageSequenceNumberList: [ 0 , 0 , 0 , 0 , 0 ] } against * end "ul_IntegProtActivationInfo" of type IntegrityProtActivationInfo end "securityModeComplete" of type SecurityModeComplete end "message" of type UL_DCCH_MessageType end "uL_DCCH_Message" of type UL_DCCH_Message end "aM_message" of type CHOICE end "car_RRC_SecModeCmpl" of type RLC_AM_DATA_IND Assignment:TSP2: [34] uL_Integrity := { rrc_MessageSequenceNumberList: [ 0 , 0 , 0 , 0 , 0 ] } Receive event:TSP2: [34] AM ? RLC_AM_DATA_IND = PDU (view PDU) Preliminary verdict:TSP2: [34] (PASS) Attach:[35] Enter Test Step ts_CRLC_UL_Integrity( { rrc_MessageSequenceNumberList: [ 0 , 0 , 0 , 0 , 0 ] } )
| 00:00:43.070 - Primitive: CRLC_Integrity_Activate_REQ 00:00:43.070 - Primitive: CRLC_Integrity_Activate_REQ Send event:[1] CRLC ! CRLC_Integrity_Activate_REQ = PDU (view PDU) 00:00:43.090 - Primitive: CRLC_Integrity_Activate_CNF begin "ca_CRLC_IntegrityActivateCnf" of type CRLC_Integrity_Activate_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER end "ca_CRLC_IntegrityActivateCnf" of type CRLC_Integrity_Activate_CNF Receive event:[2] CRLC ? CRLC_Integrity_Activate_CNF = PDU: { cellId: -1 } Attach:[35] Exit Test Step ts_CRLC_UL_Integrity
Attach:[6] Exit Test Step ts_RRC_Security::lt_StartSecurity_UE
Attach:[46] Exit Test Step ts_RRC_Security
Attach:[47] Enter Test Step ts_GMM_IdleUpdated::lt_LocUpdAcc( 0 )
| 00:00:43.090 - Primitive: RRC_DATA_REQ: mm:locationUpdatingAccept 00:00:43.090 - Primitive: RLC_AM_DATA_REQ:downlinkDirectTransfer Send event:[95] Dc ! RRC_DataReq = PDU (view PDU) 00:00:43.370 - Primitive: RLC_AM_DATA_IND: uplinkDirectTransfer 00:00:43.370 - Primitive: RRC_DATA_IND: mm:tmsiReallocationComplete begin "car_UplinkDirectTransfer" of type RRC_DataInd (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "rB_Id" of type SS_RB_Identity (INTEGER) [UNIVERSAL 2] matching 3 against 3 end "rB_Id" of type SS_RB_Identity begin "cN_Domain" of type SS_CN_DomainIdentity (INTEGER) [UNIVERSAL 2] matching 0 against 0 end "cN_Domain" of type SS_CN_DomainIdentity begin "msg" of type TMSIREALLOCATIONCOMPLETE (SEQUENCE) [UNIVERSAL 16] begin "skipIndicator" of type SkipIndicator (BITSTRING) [UNIVERSAL 3] matching '0000'B against '0000'B end "skipIndicator" of type SkipIndicator begin "mMProtocolDiscriminator" of type ProtocolDiscriminator (BITSTRING) [UNIVERSAL 3] matching '0101'B against '0101'B end "mMProtocolDiscriminator" of type ProtocolDiscriminator begin "msgType" of type MsgType (BITSTRING) [UNIVERSAL 3] matching '10011011'B against '??011011'B end "msgType" of type MsgType end "msg" of type TMSIREALLOCATIONCOMPLETE end "car_UplinkDirectTransfer" of type RRC_DataInd Receive event:[96] Dc ? RRC_DataInd = PDU (view PDU) Attach:[47] Exit Test Step ts_GMM_IdleUpdated::lt_LocUpdAcc
Attach:[48] Enter Test Step ts_GMM_IdleUpdated::lt_HandleAttachRequest( 0 )
| Assignment:[53] tcv_GMM_AttachExpect := GcFALSE Attach:[48] Exit Test Step ts_GMM_IdleUpdated::lt_HandleAttachRequest
Attach:[49] Enter Test Step ts_GMM_Authentication( 0 )
| Attach:[1] Enter Test Step ts_GMM_AuthenticationInit( )
| Attach:[1] Enter Test Step ts_GMM_AuthenticationInit::lt_IncrementCiphKeySeqNum( )
| Assignment:[18] tcv_PS_KeySeq := '000'B Attach:[1] Exit Test Step ts_GMM_AuthenticationInit::lt_IncrementCiphKeySeqNum
Attach:[2] Enter Test Step ts_GMM_AuthenticationInit::lt_AuthCalcAUTN( )
| Assignment:[19] tcv_AuthXDOUT := (view Assignment) Assignment:[20] tcv_AuthCDOUT := '0000000000000000000000000000000000000000000000000000000000000000'B Assignment:[21] tcv_AuthXDOUT_Half := '0101010101000100011101110110011000010001000000000011001100100010'B Assignment:[22] tcv_AuthAK := '011001100001000100000000001100110010001011011101'B Assignment:[23] tcv_AuthAUTN_1 := '011001100001000100000000001100110010001011011101'B Assignment:[24] tcv_AuthMAC := '0101010101000100011101110110011000010001000000000011001100100010'B Assignment:[25] tcv_AuthAUTN_2 := (view Assignment) Assignment:[26] tcv_AuthAUTN := (view Assignment) Attach:[2] Exit Test Step ts_GMM_AuthenticationInit::lt_AuthCalcAUTN
Attach:[3] Enter Test Step ts_GMM_AuthenticationInit::lt_AuthCalcUMTS_Others( )
| Assignment:[27] tcv_PS_AuthIK := (view Assignment) Assignment:[28] tcv_PS_AuthCK := (view Assignment) Assignment:[29] tcv_AuthXRES := (view Assignment) Attach:[3] Exit Test Step ts_GMM_AuthenticationInit::lt_AuthCalcUMTS_Others
Attach:[4] Enter Test Step ts_GMM_AuthenticationInit::lt_AuthCalcKcGSM( )
| Assignment:[30] tcv_AuthCK_1 := '0100010001110111011001100001000100000000001100110010001011011101'B Assignment:[31] tcv_AuthCK_2 := '1100110011111111111011101001100110001000101110111010101001010101'B Assignment:[32] tcv_AuthIK_1 := '0111011101100110000100010000000000110011001000101101110111001100'B Assignment:[33] tcv_AuthIK_2 := '1111111111101110100110011000100010111011101010100101010101000100'B Assignment:[34] tcv_AuthCK_XOR := '1000100010001000100010001000100010001000100010001000100010001000'B Assignment:[35] tcv_AuthIK_XOR := '1000100010001000100010001000100010001000100010001000100010001000'B Assignment:[36] tcv_AuthKcGSM := '0000000000000000000000000000000000000000000000000000000000000000'B Attach:[4] Exit Test Step ts_GMM_AuthenticationInit::lt_AuthCalcKcGSM
Attach:[1] Exit Test Step ts_GMM_AuthenticationInit
00:00:43.380 - Primitive: RRC_DATA_REQ: gmm:authenticationAndCipheringRequest 00:00:43.380 - Primitive: RLC_AM_DATA_REQ:downlinkDirectTransfer Send event:[2] Dc ! RRC_DataReq = PDU (view PDU) 00:00:43.850 - Primitive: RLC_AM_DATA_IND: uplinkDirectTransfer 00:00:43.850 - Primitive: RRC_DATA_IND: gmm:authenticationAndCipheringResponse begin "car_PS_UplinkDirectTransfer" of type RRC_DataInd (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "rB_Id" of type SS_RB_Identity (INTEGER) [UNIVERSAL 2] matching 3 against 3 end "rB_Id" of type SS_RB_Identity begin "cN_Domain" of type SS_CN_DomainIdentity (INTEGER) [UNIVERSAL 2] matching 1 against 1 end "cN_Domain" of type SS_CN_DomainIdentity begin "msg" of type AUTHENTICATIONANDCIPHERINGRESPONSE (SEQUENCE) [UNIVERSAL 16] begin "skipIndicator" of type SkipIndicator (BITSTRING) [UNIVERSAL 3] matching '0000'B against '0000'B end "skipIndicator" of type SkipIndicator begin "gMMProtocolDiscriminator" of type ProtocolDiscriminator (BITSTRING) [UNIVERSAL 3] matching '1000'B against '1000'B end "gMMProtocolDiscriminator" of type ProtocolDiscriminator begin "msgType" of type MsgType (BITSTRING) [UNIVERSAL 3] matching '00010011'B against '00010011'B end "msgType" of type MsgType begin "spare4" of type B4 (BITSTRING) [UNIVERSAL 3] matching '0000'B against '0000'B end "spare4" of type B4 begin "acRefNo" of type AC_ReferenceNumber (SEQUENCE) [UNIVERSAL 16] matching { value: '0011'B } against ? end "acRefNo" of type AC_ReferenceNumber begin "authRsp" of type AuthRsp_tv (SEQUENCE) [UNIVERSAL 16] begin "iei" of type IEI8 (BITSTRING) [UNIVERSAL 3] matching '00100010'B against '00100010'B end "iei" of type IEI8 begin "value" of type BITSTRING [UNIVERSAL 3] matching '01010101010001000111011101100110'B against ? end "value" of type BITSTRING end "authRsp" of type AuthRsp_tv begin "authRspExt" of type AuthRspExt (SEQUENCE) [UNIVERSAL 16] begin "iei" of type IEI8 (BITSTRING) [UNIVERSAL 3] matching '00101001'B against '00101001'B end "iei" of type IEI8 begin "iel" of type Length (OCTETSTRING) [UNIVERSAL 4] matching '04'O against ? end "iel" of type Length begin "rES" of type BITSTRING [UNIVERSAL 3] matching '00010001000000000011001100100010'B against ? end "rES" of type BITSTRING end "authRspExt" of type AuthRspExt end "msg" of type AUTHENTICATIONANDCIPHERINGRESPONSE end "car_PS_UplinkDirectTransfer" of type RRC_DataInd Assignment:[3] tcv_TmpAuthAndCiphRspPDU (view PDU) Assignment:[3] tcv_AuthRsp := '01010101010001000111011101100110'B Assignment:[3] tcv_AuthRspExt := { iei: '00101001'B , iel: '04'O , rES: '00010001000000000011001100100010'B } Receive event:[3] Dc ? RRC_DataInd = PDU (view PDU) Assignment:[4] tcv_Res := GcTRUE Preliminary verdict:TSP1: [6] (PASS) Attach:[49] Exit Test Step ts_GMM_Authentication
Attach:[50] Enter Test Step ts_GMM_IdleUpdated::lt_SecurityMode( 0 )
| Attach:[100] Enter Test Step ts_RRC_Security( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[2] Enter Test Step ts_RRC_Security::lt_RRC_InitVariables( 0 )
| Attach:[53] Enter Test Step ts_RRC_Security::lt_InitCipherMode( 0 )
| Assignment:[82] cs_cipheringStarted := GcFALSE Assignment:[82] ps_cipheringStarted := GcFALSE Assignment:[84] cipheringAlgorithmCapability := '0000000000000011'B Attach:[53] Exit Test Step ts_RRC_Security::lt_InitCipherMode
Attach:[54] Enter Test Step ts_RRC_Security::lt_InitIntegrity( 0 )
| Assignment:[87] recentSecureDomain := ps_domain Attach:[89] Enter Test Step ts_GetRRC_MessageSN( 0 )
| 00:00:43.850 - Primitive: CRLC_RRC_MessageSN_REQ Send event:[1] CRLC ! CRLC_RRC_MessageSN_REQ = PDU: { cellId: -1 , routingInfo: [rB_Identity: 0 ]} 00:00:43.870 - Primitive: CRLC_RRC_MessageSN_CNF begin "car_CRLC_RRC_MessageSN_CNF" of type CRLC_RRC_MessageSN_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "count_I_MSB_UL" of type COUNT_I_MSB (INTEGER) [UNIVERSAL 2] matching 0 against ? end "count_I_MSB_UL" of type COUNT_I_MSB begin "count_I_LSB_UL" of type RRC_SequenceNumber (INTEGER) [UNIVERSAL 2] matching 0 against ? end "count_I_LSB_UL" of type RRC_SequenceNumber begin "count_I_MSB_DL" of type COUNT_I_MSB (INTEGER) [UNIVERSAL 2] matching 0 against ? end "count_I_MSB_DL" of type COUNT_I_MSB begin "count_I_LSB_DL" of type RRC_SequenceNumber (INTEGER) [UNIVERSAL 2] matching 0 against ? end "count_I_LSB_DL" of type RRC_SequenceNumber end "car_CRLC_RRC_MessageSN_CNF" of type CRLC_RRC_MessageSN_CNF Assignment:[2] tcv_RRC_MSN_RB0 := 0 Receive event:[2] CRLC ? CRLC_RRC_MessageSN_CNF = PDU (view PDU) 00:00:43.870 - Primitive: CRLC_RRC_MessageSN_REQ Send event:[3] CRLC ! CRLC_RRC_MessageSN_REQ = PDU: { cellId: -1 , routingInfo: [rB_Identity: 1 ]} 00:00:43.880 - Primitive: CRLC_RRC_MessageSN_CNF begin "car_CRLC_RRC_MessageSN_CNF" of type CRLC_RRC_MessageSN_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "count_I_MSB_UL" of type COUNT_I_MSB (INTEGER) [UNIVERSAL 2] matching 0 against ? end "count_I_MSB_UL" of type COUNT_I_MSB begin "count_I_LSB_UL" of type RRC_SequenceNumber (INTEGER) [UNIVERSAL 2] matching 0 against ? end "count_I_LSB_UL" of type RRC_SequenceNumber begin "count_I_MSB_DL" of type COUNT_I_MSB (INTEGER) [UNIVERSAL 2] matching 0 against ? end "count_I_MSB_DL" of type COUNT_I_MSB begin "count_I_LSB_DL" of type RRC_SequenceNumber (INTEGER) [UNIVERSAL 2] matching 0 against ? end "count_I_LSB_DL" of type RRC_SequenceNumber end "car_CRLC_RRC_MessageSN_CNF" of type CRLC_RRC_MessageSN_CNF Assignment:[4] tcv_RRC_MSN_RB1 := 0 Receive event:[4] CRLC ? CRLC_RRC_MessageSN_CNF = PDU (view PDU) 00:00:43.880 - Primitive: CRLC_RRC_MessageSN_REQ Send event:[5] CRLC ! CRLC_RRC_MessageSN_REQ = PDU: { cellId: -1 , routingInfo: [rB_Identity: 2 ]} 00:00:43.900 - Primitive: CRLC_RRC_MessageSN_CNF begin "car_CRLC_RRC_MessageSN_CNF" of type CRLC_RRC_MessageSN_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "count_I_MSB_UL" of type COUNT_I_MSB (INTEGER) [UNIVERSAL 2] matching 0 against ? end "count_I_MSB_UL" of type COUNT_I_MSB begin "count_I_LSB_UL" of type RRC_SequenceNumber (INTEGER) [UNIVERSAL 2] matching 1 against ? end "count_I_LSB_UL" of type RRC_SequenceNumber begin "count_I_MSB_DL" of type COUNT_I_MSB (INTEGER) [UNIVERSAL 2] matching 0 against ? end "count_I_MSB_DL" of type COUNT_I_MSB begin "count_I_LSB_DL" of type RRC_SequenceNumber (INTEGER) [UNIVERSAL 2] matching 1 against ? end "count_I_LSB_DL" of type RRC_SequenceNumber end "car_CRLC_RRC_MessageSN_CNF" of type CRLC_RRC_MessageSN_CNF Assignment:[6] tcv_RRC_MSN_RB2 := 1 Assignment:[6] tcv_RRC_MSN_RB2_UL := 1 Receive event:[6] CRLC ? CRLC_RRC_MessageSN_CNF = PDU (view PDU) 00:00:43.900 - Primitive: CRLC_RRC_MessageSN_REQ Send event:[7] CRLC ! CRLC_RRC_MessageSN_REQ = PDU: { cellId: -1 , routingInfo: [rB_Identity: 3 ]} 00:00:43.920 - Primitive: CRLC_RRC_MessageSN_CNF begin "car_CRLC_RRC_MessageSN_CNF" of type CRLC_RRC_MessageSN_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "count_I_MSB_UL" of type COUNT_I_MSB (INTEGER) [UNIVERSAL 2] matching 0 against ? end "count_I_MSB_UL" of type COUNT_I_MSB begin "count_I_LSB_UL" of type RRC_SequenceNumber (INTEGER) [UNIVERSAL 2] matching 2 against ? end "count_I_LSB_UL" of type RRC_SequenceNumber begin "count_I_MSB_DL" of type COUNT_I_MSB (INTEGER) [UNIVERSAL 2] matching 0 against ? end "count_I_MSB_DL" of type COUNT_I_MSB begin "count_I_LSB_DL" of type RRC_SequenceNumber (INTEGER) [UNIVERSAL 2] matching 2 against ? end "count_I_LSB_DL" of type RRC_SequenceNumber end "car_CRLC_RRC_MessageSN_CNF" of type CRLC_RRC_MessageSN_CNF Assignment:[8] tcv_RRC_MSN_RB3 := 2 Receive event:[8] CRLC ? CRLC_RRC_MessageSN_CNF = PDU (view PDU) 00:00:43.920 - Primitive: CRLC_RRC_MessageSN_REQ Send event:[9] CRLC ! CRLC_RRC_MessageSN_REQ = PDU: { cellId: -1 , routingInfo: [rB_Identity: 4 ]} 00:00:43.930 - Primitive: CRLC_RRC_MessageSN_CNF begin "car_CRLC_RRC_MessageSN_CNF" of type CRLC_RRC_MessageSN_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "count_I_MSB_UL" of type COUNT_I_MSB (INTEGER) [UNIVERSAL 2] matching 0 against ? end "count_I_MSB_UL" of type COUNT_I_MSB begin "count_I_LSB_UL" of type RRC_SequenceNumber (INTEGER) [UNIVERSAL 2] matching 0 against ? end "count_I_LSB_UL" of type RRC_SequenceNumber begin "count_I_MSB_DL" of type COUNT_I_MSB (INTEGER) [UNIVERSAL 2] matching 0 against ? end "count_I_MSB_DL" of type COUNT_I_MSB begin "count_I_LSB_DL" of type RRC_SequenceNumber (INTEGER) [UNIVERSAL 2] matching 0 against ? end "count_I_LSB_DL" of type RRC_SequenceNumber end "car_CRLC_RRC_MessageSN_CNF" of type CRLC_RRC_MessageSN_CNF Assignment:[10] tcv_RRC_MSN_RB4 := 0 Receive event:[10] CRLC ? CRLC_RRC_MessageSN_CNF = PDU (view PDU) Attach:[89] Exit Test Step ts_GetRRC_MessageSN
Assignment:[90] dL_Integrity := (view Assignment) Assignment:[90] tcv_Int_ModifyFlag := GcTRUE Attach:[54] Exit Test Step ts_RRC_Security::lt_InitIntegrity
Attach:[55] Enter Test Step ts_InitSystemSpecificCap( )
| Assignment:[11] tcv_UE_SystemSpecificCap := 0 Attach:[55] Exit Test Step ts_InitSystemSpecificCap
Attach:[56] Enter Test Step ts_SaveCellInfo( 0 )
| Assignment:[2] tcv_CellInfoA := (view Assignment) Attach:[56] Exit Test Step ts_SaveCellInfo
Assignment:[58] tcv_HFN := '00000000000000000000'B Assignment:[62] start_PS := '00000000000000000000'B Attach:[2] Exit Test Step ts_RRC_Security::lt_RRC_InitVariables
Attach:[3] Enter Test Step ts_SS_DownloadSecurityKey( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[15] Enter Test Step ts_SS_DownloadSecurityKey::lt_DownloadKeyCRLC( '00000000000000000000'B )
| 00:00:43.930 - Primitive: CRLC_SecurityMode_Config_REQ 00:00:43.930 - Primitive: CRLC_SecurityMode_Config_REQ Send event:[21] CRLC ! CRLC_SecurityMode_Config_REQ = PDU (view PDU) 00:00:43.950 - Primitive: CRLC_SecurityMode_Config_CNF begin "ca_CRLC_SecurityModeCfgCnf" of type CRLC_SecurityMode_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER end "ca_CRLC_SecurityModeCfgCnf" of type CRLC_SecurityMode_Config_CNF Receive event:[22] CRLC ? CRLC_SecurityMode_Config_CNF = PDU: { cellId: -1 } Attach:[15] Exit Test Step ts_SS_DownloadSecurityKey::lt_DownloadKeyCRLC
Attach:[3] Exit Test Step ts_SS_DownloadSecurityKey
Attach:[4] Enter Test Step ts_RRC_Security::lt_ActivateSecurity_DL_SS( 0 )
| Attach:[14] Enter Test Step ts_RRC_Security::lt_InitialiseRRC_MSN( 0 )
| Attach:[14] Exit Test Step ts_RRC_Security::lt_InitialiseRRC_MSN
Attach:[15] Enter Test Step ts_CRLC_DL_Integrity( { integrityProtectionM ...
| (view Test Step parameters) 00:00:43.950 - Primitive: CRLC_Integrity_Activate_REQ 00:00:43.950 - Primitive: CRLC_Integrity_Activate_REQ Send event:[1] CRLC ! CRLC_Integrity_Activate_REQ = PDU (view PDU) 00:00:43.960 - Primitive: CRLC_Integrity_Activate_CNF begin "ca_CRLC_IntegrityActivateCnf" of type CRLC_Integrity_Activate_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER end "ca_CRLC_IntegrityActivateCnf" of type CRLC_Integrity_Activate_CNF Receive event:[2] CRLC ? CRLC_Integrity_Activate_CNF = PDU: { cellId: -1 } Attach:[15] Exit Test Step ts_CRLC_DL_Integrity
Attach:[4] Exit Test Step ts_RRC_Security::lt_ActivateSecurity_DL_SS
Attach:[5] Enter Test Step ts_RRC_Security::lt_RB2_UL_IntegrityActivate( 0 )
| Attach:[11] Enter Test Step ts_RB2_UL_IntegrityActivate( 1 )
| 00:00:43.960 - Primitive: CRLC_Integrity_Activate_REQ 00:00:43.960 - Primitive: CRLC_Integrity_Activate_REQ Send event:[1] CRLC ! CRLC_Integrity_Activate_REQ = PDU (view PDU) 00:00:43.980 - Primitive: CRLC_Integrity_Activate_CNF begin "ca_CRLC_IntegrityActivateCnf" of type CRLC_Integrity_Activate_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER end "ca_CRLC_IntegrityActivateCnf" of type CRLC_Integrity_Activate_CNF Receive event:[2] CRLC ? CRLC_Integrity_Activate_CNF = PDU: { cellId: -1 } Attach:[11] Exit Test Step ts_RB2_UL_IntegrityActivate
Attach:[5] Exit Test Step ts_RRC_Security::lt_RB2_UL_IntegrityActivate
Attach:[6] Enter Test Step ts_RRC_Security::lt_StartSecurity_UE( 0 )
| Attach:[27] Enter Test Step ts_RRC_Security::lt_SendSecurityModeCommand( 0 )
| 00:00:43.980 - Primitive: RLC_AM_DATA_REQ 00:00:43.980 - Primitive: RLC_AM_DATA_REQ: securityModeCommand Send event:[52] AM ! RLC_AM_DATA_REQ = PDU (view PDU) Attach:[27] Exit Test Step ts_RRC_Security::lt_SendSecurityModeCommand
00:00:44.280 - Primitive: RLC_AM_DATA_IND: securityModeComplete 00:00:44.280 - Primitive: RLC_AM_DATA_IND begin "car_RRC_SecModeCmpl" of type RLC_AM_DATA_IND (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "integrityResult" of type IntegrityResult (CHOICE) [UNIVERSAL 31] matching [integrityUsed: i_pass] against * end "integrityResult" of type IntegrityResult begin "aM_message" of type CHOICE [UNIVERSAL 31] begin "uL_DCCH_Message" of type UL_DCCH_Message (SEQUENCE) [UNIVERSAL 16] begin "integrityCheckInfo" of type IntegrityCheckInfo (SEQUENCE) [UNIVERSAL 16] matching { messageAuthenticationCode: '11100000000110011010110001001011'B , rrc_MessageSequenceNumber: 2 } against * end "integrityCheckInfo" of type IntegrityCheckInfo begin "message" of type UL_DCCH_MessageType (CHOICE) [UNIVERSAL 31] begin "securityModeComplete" of type SecurityModeComplete (SEQUENCE) [UNIVERSAL 16] begin "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier (INTEGER) [UNIVERSAL 2] matching 0 against 0 end "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier begin "ul_IntegProtActivationInfo" of type IntegrityProtActivationInfo (SEQUENCE) [UNIVERSAL 16] matching { rrc_MessageSequenceNumberList: [ 5 , 1 , 2 , 3 , 1 ] } against * end "ul_IntegProtActivationInfo" of type IntegrityProtActivationInfo end "securityModeComplete" of type SecurityModeComplete end "message" of type UL_DCCH_MessageType end "uL_DCCH_Message" of type UL_DCCH_Message end "aM_message" of type CHOICE end "car_RRC_SecModeCmpl" of type RLC_AM_DATA_IND Assignment:TSP2: [34] uL_Integrity := { rrc_MessageSequenceNumberList: [ 5 , 1 , 2 , 3 , 1 ] } Receive event:TSP2: [34] AM ? RLC_AM_DATA_IND = PDU (view PDU) Preliminary verdict:TSP2: [34] (PASS) Attach:[35] Enter Test Step ts_CRLC_UL_Integrity( { rrc_MessageSequenceNumberList: [ 5 , 1 , 2 , 3 , 1 ] } )
| 00:00:44.280 - Primitive: CRLC_Integrity_Activate_REQ 00:00:44.280 - Primitive: CRLC_Integrity_Activate_REQ Send event:[1] CRLC ! CRLC_Integrity_Activate_REQ = PDU (view PDU) 00:00:44.290 - Primitive: CRLC_Integrity_Activate_CNF begin "ca_CRLC_IntegrityActivateCnf" of type CRLC_Integrity_Activate_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER end "ca_CRLC_IntegrityActivateCnf" of type CRLC_Integrity_Activate_CNF Receive event:[2] CRLC ? CRLC_Integrity_Activate_CNF = PDU: { cellId: -1 } Attach:[35] Exit Test Step ts_CRLC_UL_Integrity
Attach:[6] Exit Test Step ts_RRC_Security::lt_StartSecurity_UE
Attach:[100] Exit Test Step ts_RRC_Security
Attach:[50] Exit Test Step ts_GMM_IdleUpdated::lt_SecurityMode
Attach:[51] Enter Test Step ts_GMM_IdleUpdated::lt_AttachAccept( 0 )
| Assignment:[110] tcv_AssignedPTMSI := '12345678'O Assignment:[110] tcv_Assigned_PTMSI_Sig := 'AB1234'O 00:00:44.290 - Primitive: RRC_DATA_REQ: gmm:attachAccept 00:00:44.290 - Primitive: RLC_AM_DATA_REQ:downlinkDirectTransfer Send event:[112] Dc ! RRC_DataReq = PDU (view PDU) 00:00:44.570 - Primitive: RLC_AM_DATA_IND: uplinkDirectTransfer 00:00:44.570 - Primitive: RRC_DATA_IND: gmm:attachComplete begin "car_PS_UplinkDirectTransfer" of type RRC_DataInd (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "rB_Id" of type SS_RB_Identity (INTEGER) [UNIVERSAL 2] matching 3 against 3 end "rB_Id" of type SS_RB_Identity begin "cN_Domain" of type SS_CN_DomainIdentity (INTEGER) [UNIVERSAL 2] matching 1 against 1 end "cN_Domain" of type SS_CN_DomainIdentity begin "msg" of type ATTACHCOMPLETE (SEQUENCE) [UNIVERSAL 16] begin "skipIndicator" of type SkipIndicator (BITSTRING) [UNIVERSAL 3] matching '0000'B against '0000'B end "skipIndicator" of type SkipIndicator begin "gMMProtocolDiscriminator" of type ProtocolDiscriminator (BITSTRING) [UNIVERSAL 3] matching '1000'B against '1000'B end "gMMProtocolDiscriminator" of type ProtocolDiscriminator begin "msgType" of type MsgType (BITSTRING) [UNIVERSAL 3] matching '00000011'B against '00000011'B end "msgType" of type MsgType end "msg" of type ATTACHCOMPLETE end "car_PS_UplinkDirectTransfer" of type RRC_DataInd Receive event:[113] Dc ? RRC_DataInd = PDU (view PDU) Attach:[51] Exit Test Step ts_GMM_IdleUpdated::lt_AttachAccept
Attach:[52] Enter Test Step ts_GMM_IdleUpdated::lt_RRC_ConnRel( 0 )
| Attach:[120] Enter Test Step ts_RRC_ConnRel( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[2] Enter Test Step ts_RRC_Delay( 1000 )
| StartTimer:[1] t_Dly [5000] 1000 ms Timed out Timer:t_Dly TimeOut:[2] t_Dly [5000] 1000 ms Attach:[2] Exit Test Step ts_RRC_Delay
Attach:[3] Enter Test Step ts_RRC_ConnRel::lt_Send_RRC_ConnectionRelease( 0 )
| Assignment:[39] tcv_N308 := 1 Assignment:[39] tcv_K := 1 00:00:45.600 - Primitive: RLC_UM_DATA_REQ 00:00:45.600 - Primitive: RLC_UM_DATA_REQ: rrcConnectionRelease Send event:[40] UM ! RLC_UM_DATA_REQ = PDU (view PDU) 00:00:45.870 - Primitive: RLC_UM_DATA_IND: rrcConnectionReleaseComplete 00:00:45.870 - Primitive: RLC_UM_DATA_IND begin "car_RRC_ConnRelCmplUM" of type RLC_UM_DATA_IND (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "integrityResult" of type IntegrityResult (CHOICE) [UNIVERSAL 31] matching [integrityUsed: i_pass] against * end "integrityResult" of type IntegrityResult begin "uM_message" of type CHOICE [UNIVERSAL 31] begin "uL_DCCH_Message" of type UL_DCCH_Message (SEQUENCE) [UNIVERSAL 16] begin "integrityCheckInfo" of type IntegrityCheckInfo (SEQUENCE) [UNIVERSAL 16] matching { messageAuthenticationCode: '11110111111000101100001011001110'B , rrc_MessageSequenceNumber: 1 } against * end "integrityCheckInfo" of type IntegrityCheckInfo begin "message" of type UL_DCCH_MessageType (CHOICE) [UNIVERSAL 31] begin "rrcConnectionReleaseComplete" of type RRCConnectionReleaseComplete (SEQUENCE) [UNIVERSAL 16] begin "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier (INTEGER) [UNIVERSAL 2] matching 0 against 0 end "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier end "rrcConnectionReleaseComplete" of type RRCConnectionReleaseComplete end "message" of type UL_DCCH_MessageType end "uL_DCCH_Message" of type UL_DCCH_Message end "uM_message" of type CHOICE end "car_RRC_ConnRelCmplUM" of type RLC_UM_DATA_IND Receive event:TSP1: [41] UM ? RLC_UM_DATA_IND = PDU (view PDU) Preliminary verdict:TSP1: [41] (PASS) Attach:[42] Enter Test Step ts_RRC_ConnRel::lt_RptRcvConnRel( 0 )
| StartTimer:[50] t_Dly [5000] 5000 ms 00:00:46.040 - Primitive: RLC_UM_DATA_IND: rrcConnectionReleaseComplete 00:00:46.040 - Primitive: RLC_UM_DATA_IND begin "car_RRC_ConnRelCmplUM" of type RLC_UM_DATA_IND (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "integrityResult" of type IntegrityResult (CHOICE) [UNIVERSAL 31] matching [integrityUsed: i_pass] against * end "integrityResult" of type IntegrityResult begin "uM_message" of type CHOICE [UNIVERSAL 31] begin "uL_DCCH_Message" of type UL_DCCH_Message (SEQUENCE) [UNIVERSAL 16] begin "integrityCheckInfo" of type IntegrityCheckInfo (SEQUENCE) [UNIVERSAL 16] matching { messageAuthenticationCode: '10111001101000110000011111000000'B , rrc_MessageSequenceNumber: 2 } against * end "integrityCheckInfo" of type IntegrityCheckInfo begin "message" of type UL_DCCH_MessageType (CHOICE) [UNIVERSAL 31] begin "rrcConnectionReleaseComplete" of type RRCConnectionReleaseComplete (SEQUENCE) [UNIVERSAL 16] begin "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier (INTEGER) [UNIVERSAL 2] matching 0 against 0 end "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier end "rrcConnectionReleaseComplete" of type RRCConnectionReleaseComplete end "message" of type UL_DCCH_MessageType end "uL_DCCH_Message" of type UL_DCCH_Message end "uM_message" of type CHOICE end "car_RRC_ConnRelCmplUM" of type RLC_UM_DATA_IND Assignment:TSP2: [53] tcv_K := 2 CancelTimer:TSP2: [53] t_Dly [5000] 5000 ms Receive event:TSP2: [53] UM ? RLC_UM_DATA_IND = PDU (view PDU) Preliminary verdict:TSP2: [53] (PASS) Attach:[42] Exit Test Step ts_RRC_ConnRel::lt_RptRcvConnRel
Attach:[3] Exit Test Step ts_RRC_ConnRel::lt_Send_RRC_ConnectionRelease
Attach:[4] Enter Test Step ts_RRC_ConnRel::lt_RestartCRLC_ForNextConnection( 0 )
| Attach:[7] Enter Test Step ts_CRLC_RelReconfSRB( 0 )
| Attach:[1] Enter Test Step ts_CRLC_Rel( -1 )
| 00:00:46.040 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:00:46.060 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 1 ]} Attach:[1] Exit Test Step ts_CRLC_Rel
Attach:[2] Enter Test Step ts_CRLC_Rel( -1 )
| 00:00:46.060 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:00:46.070 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 2 ]} Attach:[2] Exit Test Step ts_CRLC_Rel
Attach:[3] Enter Test Step ts_CRLC_Rel( -1 )
| 00:00:46.070 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:00:46.090 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 3 ]} Attach:[3] Exit Test Step ts_CRLC_Rel
Attach:[4] Enter Test Step ts_CRLC_Rel( -1 )
| 00:00:46.090 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:00:46.100 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 4 ]} Attach:[4] Exit Test Step ts_CRLC_Rel
Attach:[5] Enter Test Step ts_SS_RB1_ToRB4_Cfg( )
| 00:00:46.100 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:00:46.120 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 1 ]} 00:00:46.120 - Primitive: CRLC_Config_REQ Send event:[3] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:00:46.130 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[4] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 2 ]} 00:00:46.130 - Primitive: CRLC_Config_REQ Send event:[5] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:00:46.150 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[6] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 3 ]} 00:00:46.150 - Primitive: CRLC_Config_REQ Send event:[7] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:00:46.170 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[8] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 4 ]} Attach:[5] Exit Test Step ts_SS_RB1_ToRB4_Cfg
Attach:[7] Exit Test Step ts_CRLC_RelReconfSRB
Attach:[8] Enter Test Step ts_SetCellCfg( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Assignment:[2] cellConfig := cell_DCH_StandAloneSRB_NoConn Attach:[3] Enter Test Step ts_SaveCellInfo( 0 )
| Assignment:[2] tcv_CellInfoA := (view Assignment) Attach:[3] Exit Test Step ts_SaveCellInfo
Attach:[8] Exit Test Step ts_SetCellCfg
Attach:[4] Exit Test Step ts_RRC_ConnRel::lt_RestartCRLC_ForNextConnection
Attach:[5] Enter Test Step ts_SS_ResetSecurityKey( )
| Assignment:[1] tcv_CellIndInfo := (view Assignment) Assignment:[3] cipheringAlgorithmCapability := '0000000000000011'B Attach:[5] Exit Test Step ts_SS_ResetSecurityKey
Attach:[120] Exit Test Step ts_RRC_ConnRel
Attach:[52] Exit Test Step ts_GMM_IdleUpdated::lt_RRC_ConnRel
Attach:[6] Exit Test Step ts_GMM_IdleUpdated::lt_IdleUpdated_NMO_II
Assignment:[7] tcv_Use_E_PLMN := GcFALSE Attach:[2] Exit Test Step ts_GMM_IdleUpdated
Attach:[6] Exit Test Step ts_IdleUpdated
Assignment:[7] attFlag := 0 Assignment:[7] t3212 := '00'O Attach:[8] Enter Test Step ts_SysInfoModifyMM( 0 )
| Assignment:[2] mcc := [ 0 , 0 , 1 ] Assignment:[2] mnc := [ 0 , 1 ] Assignment:[3] cn_CommonGSM_MAP_NAS_SysInfo := '0001'O Assignment:[3] gsm_MAP := '0000'O Assignment:[3] gsm_MAP := '0501'O Attach:[4] Enter Test Step ts_SendSIB1( { cn_CommonGSM_MAP_NAS ...
| (view Test Step parameters) Assignment:[1] tcv_SIB1 := (view Assignment) 00:00:46.170 - Primitive: o_SIB_PER_Encoding Assignment:[1] seg1 := (view Assignment) 00:00:46.170 - Primitive: o_SIB_PER_Encoding Assignment:[1] seg2 := '00000000000000000001'B Attach:[4] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:46.170 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[4] Exit Test Step ts_Scheduling
00:00:46.180 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[5] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} 00:00:46.180 - Primitive: RLC_TR_DATA_REQ 00:00:46.180 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[6] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Assignment:[7] sysInfoType1 := 4 Attach:[8] Enter Test Step ts_ChangeMIB_ValueTag( )
| Assignment:[2] mib_ValueTag := 3 Assignment:[2] tcv_MIB_ValueTagChanged := GcTRUE Attach:[8] Exit Test Step ts_ChangeMIB_ValueTag
Attach:[4] Exit Test Step ts_SendSIB1
Attach:[5] Enter Test Step ts_SendMIB( { mib_ValueTag: 3 , pl ...
| (view Test Step parameters) Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Assignment:[2] mcc := [ 0 , 0 , 1 ] Assignment:[2] mnc := [ 0 , 1 ] 00:00:46.180 - Primitive: o_SIB_PER_Encoding Assignment:[3] tcv_Segs := (view Assignment) Attach:[6] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:46.180 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[6] Exit Test Step ts_Scheduling
00:00:46.200 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[7] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} Attach:[8] Enter Test Step ts_SendMIB::lt_CompleteSIB( masterInformationBlock )
| 00:00:46.200 - Primitive: RLC_TR_DATA_REQ 00:00:46.200 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[13] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[8] Exit Test Step ts_SendMIB::lt_CompleteSIB
Assignment:[9] tcv_MIB_ValueTagChanged := GcFALSE Attach:[5] Exit Test Step ts_SendMIB
Attach:[6] Enter Test Step ts_SendPage1_ModifySI( 0 )
| Attach:[1] Enter Test Step ts_RRC_Delay( 5000 )
| StartTimer:[1] t_Dly [5000] 5000 ms Timed out Timer:t_Dly TimeOut:[2] t_Dly [5000] 5000 ms Attach:[1] Exit Test Step ts_RRC_Delay
Attach:[2] Enter Test Step ts_CMAC_Pag1_Cfg( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[3] Enter Test Step ts_CMAC_Pag1_Cfg::lt_CalculateDrxCycleLength( 0 )
| Assignment:[10] tcv_dRX_CycleLengthPaging := 7 Attach:[3] Exit Test Step ts_CMAC_Pag1_Cfg::lt_CalculateDrxCycleLength
00:00:51.210 - Primitive: CMAC_PAGING_Config_REQ Send event:[4] CMAC ! CMAC_PAGING_Config_REQ = PDU (view PDU) 00:00:51.230 - Primitive: CMAC_PAGING_Config_CNF begin "ca_CMAC_PagingCfgCnf" of type CMAC_PAGING_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 5 against 5 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_PagingCfgCnf" of type CMAC_PAGING_Config_CNF Receive event:[5] CMAC ? CMAC_PAGING_Config_CNF = PDU (view PDU) Attach:[2] Exit Test Step ts_CMAC_Pag1_Cfg
00:00:51.230 - Primitive: RLC_TR_DATA_REQ 00:00:51.230 - Primitive: RLC_TR_DATA_REQ: pagingType1 Send event:[3] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[4] Enter Test Step ts_SendSysInfoChangeInd_InFACHConfig( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[4] Exit Test Step ts_SendSysInfoChangeInd_InFACHConfig
Attach:[6] Exit Test Step ts_SendPage1_ModifySI
Attach:[8] Exit Test Step ts_SysInfoModifyMM
Attach:[9] Enter Test Step ts_GMM_DetachOnSwitchOff( 0 )
| Attach:[1] Enter Test Step ts_RRC_Delay( 5000 )
| StartTimer:[1] t_Dly [5000] 5000 ms Timed out Timer:t_Dly TimeOut:[2] t_Dly [5000] 5000 ms Attach:[1] Exit Test Step ts_RRC_Delay
Attach:[3] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[3] Exit Test Step ts_SetTmpCellInfo
Attach:[4] Enter Test Step ts_GMM_DetachOnSwitchOff::lt_Init_RRC_RelStatus( 0 )
| Assignment:[24] tcv_RRC_RelStatus := cell_Dch Attach:[4] Exit Test Step ts_GMM_DetachOnSwitchOff::lt_Init_RRC_RelStatus
Attach:[5] Enter Test Step ts_MMI_UE_SwitchOff( )
| 00:00:56.230 - Primitive: MMI_CmdReq Send event:[2] Ut ! MMI_CmdReq = PDU: { cmd: "Please switch off the UE" } 00:00:57.420 - Primitive: MMI_CmdCnf begin "ca_MMI_CmdCnf" of type MMI_CmdCnf (SEQUENCE) [UNIVERSAL 16] begin "result" of type BOOLEAN [UNIVERSAL 1] matching GcTRUE against GcTRUE end "result" of type BOOLEAN end "ca_MMI_CmdCnf" of type MMI_CmdCnf Receive event:[3] Ut ? MMI_CmdCnf = PDU: { result: GcTRUE , resultString: OMIT} Assignment:[4] tcv_UE_SwitchedOn := GcFALSE Attach:[5] Exit Test Step ts_MMI_UE_SwitchOff
Attach:[6] Enter Test Step ts_RRC_ConnEst( 0 )
| Attach:[1] Enter Test Step ts_SS_PrepareCellRRC_ConnEst( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[1] Exit Test Step ts_SS_PrepareCellRRC_ConnEst
Attach:[2] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[2] Exit Test Step ts_SetTmpCellInfo
Attach:[3] Enter Test Step ts_RRC_ConnEst::lt_RcvConnReq( 0 )
| 00:01:00.620 - Primitive: RLC_TR_DATA_IND: rrcConnectionRequest 00:01:00.620 - Primitive: RLC_TR_DATA_IND begin "car_RRC_ConnReq" of type RLC_TR_DATA_IND (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "tM_message" of type CHOICE [UNIVERSAL 31] begin "uL_CCCH_Message" of type UL_CCCH_Message (SEQUENCE) [UNIVERSAL 16] begin "message" of type UL_CCCH_MessageType (CHOICE) [UNIVERSAL 31] begin "rrcConnectionRequest" of type RRCConnectionRequest (SEQUENCE) [UNIVERSAL 16] begin "initialUE_Identity" of type InitialUE_Identity (CHOICE) [UNIVERSAL 31] begin InitialUE_Identity (CHOICE) [UNIVERSAL 31] end InitialUE_Identity begin InitialUE_Identity (CHOICE) [UNIVERSAL 31] begin "tmsi_and_LAI" of type TMSI_and_LAI_GSM_MAP (SEQUENCE) [UNIVERSAL 16] matching { tmsi: '00010001001000100011001101000100'B , lai: { plmn_Identity: { mcc: [ 0 , 0 , 1 ] , mnc: [ 0 , 1 ] } , lac: '0000000000000001'B } } against ? end "tmsi_and_LAI" of type TMSI_and_LAI_GSM_MAP end InitialUE_Identity matching [tmsi_and_LAI: { tmsi: '00010001001000100011001101000100'B , lai: { plmn_Identity: { mcc: [ 0 , 0 , 1 ] , mnc: [ 0 , 1 ] } , lac: '0000000000000001'B } } ] against ([imsi: ?], [tmsi_and_LAI: ?], [p_TMSI_and_RAI: ?], [imei: ?]) end "initialUE_Identity" of type InitialUE_Identity begin "establishmentCause" of type EstablishmentCause (ENUMERATED) [UNIVERSAL 10] matching detach against detach end "establishmentCause" of type EstablishmentCause begin "protocolErrorIndicator" of type ProtocolErrorIndicator (ENUMERATED) [UNIVERSAL 10] matching noError against noError end "protocolErrorIndicator" of type ProtocolErrorIndicator end "rrcConnectionRequest" of type RRCConnectionRequest end "message" of type UL_CCCH_MessageType end "uL_CCCH_Message" of type UL_CCCH_Message end "tM_message" of type CHOICE end "car_RRC_ConnReq" of type RLC_TR_DATA_IND Assignment:[9] tcv_InitialUE_Id := (view Assignment) Receive event:[9] TM ? RLC_TR_DATA_IND = PDU (view PDU) Attach:[3] Exit Test Step ts_RRC_ConnEst::lt_RcvConnReq
Attach:[4] Enter Test Step ts_RRC_ConnEst::lt_Send_ConnSetUp( 0 )
| 00:01:00.620 - Primitive: RLC_UM_DATA_REQ 00:01:00.620 - Primitive: RLC_UM_DATA_REQ: rrcConnectionSetup Send event:[31] UM ! RLC_UM_DATA_REQ = PDU (view PDU) Attach:[33] Enter Test Step ts_SetCellCfg( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Assignment:[2] cellConfig := cell_DCH_StandAloneSRB Attach:[3] Enter Test Step ts_SaveCellInfo( 0 )
| Assignment:[2] tcv_CellInfoA := (view Assignment) Attach:[3] Exit Test Step ts_SaveCellInfo
Attach:[33] Exit Test Step ts_SetCellCfg
Attach:[4] Exit Test Step ts_RRC_ConnEst::lt_Send_ConnSetUp
Attach:[5] Enter Test Step ts_RRC_ReceiveConnSetupCmpl( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
StartTimer:[3] t_WaitMS [13500] 13500 ms 00:01:01.120 - Primitive: RLC_AM_DATA_IND: rrcConnectionSetupComplete 00:01:01.120 - Primitive: RLC_AM_DATA_IND begin "car_RRC_ConnSetupCmpl" of type RLC_AM_DATA_IND (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "integrityResult" of type IntegrityResult (CHOICE) [UNIVERSAL 31] matching [integrityUsed: i_pass] against ? end "integrityResult" of type IntegrityResult begin "aM_message" of type CHOICE [UNIVERSAL 31] begin "uL_DCCH_Message" of type UL_DCCH_Message (SEQUENCE) [UNIVERSAL 16] begin "message" of type UL_DCCH_MessageType (CHOICE) [UNIVERSAL 31] begin "rrcConnectionSetupComplete" of type RRCConnectionSetupComplete (SEQUENCE) [UNIVERSAL 16] begin "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier (INTEGER) [UNIVERSAL 2] matching 0 against 0 end "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier begin "startList" of type STARTList (SEQUENCEOF) [UNIVERSAL 28] matching [ { cn_DomainIdentity: ps_domain, start_Value: '00000000000000000010'B } , { cn_DomainIdentity: cs_domain, start_Value: '00000000000000000010'B } ] against ? end "startList" of type STARTList begin "ue_RadioAccessCapability" of type UE_RadioAccessCapability (SEQUENCE) [UNIVERSAL 16] matching { accessStratumReleaseIndicator: r99, pdcp_Capability: { losslessSRNS_RelocationSupport: GcFALSE , supportForRfc2507: [notSupported: NULL]} , rlc_Capability: { totalRLC_AM_BufferSize: kb50, maximumRLC_WindowSize: mws2047, maximumAM_EntityNumber: am6} , transportChannelCapability: { dl_TransChCapability: { maxNoBitsReceived: b8960, maxConvCodeBitsReceived: b1280, turboDecodingSupport: [supported: b8960], maxSimultaneousTransChs: e8, maxSimultaneousCCTrCH_Count: 1 , maxReceivedTransportBlocks: tb32, maxNumberOfTFC: tfc128, maxNumberOfTF: tf64} , ul_TransChCapability: { maxNoBitsTransmitted: b3840, maxConvCodeBitsTransmitted: b1280, turboEncodingSupport: [supported: b3840], maxSimultaneousTransChs: e8, modeSpecificInfo: [fdd: NULL], maxTransmittedBlocks: tb32, maxNumberOfTFC: tfc64, maxNumberOfTF: tf32} } , rf_Capability: { fddRF_Capability: { ue_PowerClass: 4 , txRxFrequencySeparation: mhz190} , tddRF_Capability: OMIT} , physicalChannelCapability: { fddPhysChCapability: { downlinkPhysChCapability: { maxNoDPCH_PDSCH_Codes: 1 , maxNoPhysChBitsReceived: b9600, supportForSF_512: GcFALSE , supportOfPDSCH: GcFALSE , simultaneousSCCPCH_DPCH_Reception: [notSupported: NULL]} , uplinkPhysChCapability: { maxNoDPDCH_BitsTransmitted: b4800, supportOfPCPCH: GcFALSE } } , tddPhysChCapability: OMIT} , ue_MultiModeRAT_Capability: { multiRAT_CapabilityList: { supportOfGSM: GcFALSE , supportOfMulticarrier: GcFALSE } , multiModeCapability: fdd} , securityCapability: { cipheringAlgorithmCap: '0000000000000011'B , integrityProtectionAlgorithmCap: '0000000000000010'B } , ue_positioning_Capability: { standaloneLocMethodsSupported: GcFALSE , ue_BasedOTDOA_Supported: GcFALSE , networkAssistedGPS_Supported: noNetworkAssistedGPS, supportForUE_GPS_TimingOfCellFrames: GcFALSE , supportForIPDL: GcFALSE } , measurementCapability: { downlinkCompressedMode: { fdd_Measurements: GcTRUE , tdd_Measurements: OMIT, gsm_Measurements: { gsm900: GcTRUE , dcs1800: GcTRUE , gsm1900: GcTRUE } , multiCarrierMeasurements: GcFALSE } , uplinkCompressedMode: { fdd_Measurements: GcTRUE , tdd_Measurements: OMIT, gsm_Measurements: { gsm900: GcTRUE , dcs1800: GcTRUE , gsm1900: GcTRUE } , multiCarrierMeasurements: GcFALSE } } } against * end "ue_RadioAccessCapability" of type UE_RadioAccessCapability end "rrcConnectionSetupComplete" of type RRCConnectionSetupComplete end "message" of type UL_DCCH_MessageType end "uL_DCCH_Message" of type UL_DCCH_Message end "aM_message" of type CHOICE end "car_RRC_ConnSetupCmpl" of type RLC_AM_DATA_IND Assignment:TSP1: [5] tcv_StartList := (view Assignment) Assignment:TSP1: [5] cipheringAlgorithmCapability := '0000000000000011'B CancelTimer:TSP1: [5] t_WaitMS [13500] 13500 ms Receive event:TSP1: [5] AM ? RLC_AM_DATA_IND = PDU (view PDU) Preliminary verdict:TSP1: [5] (PASS) Attach:[6] Enter Test Step ts_RRC_ReceiveConnSetupCmpl::lt_GetHFN( 0 )
| Assignment:[13] tcv_Count := 2 Attach:[17] Enter Test Step ts_RRC_ReceiveConnSetupCmpl::lt_FirstValue( 0 )
| Assignment:[23] start_PS := '00000000000000000010'B Attach:[17] Exit Test Step ts_RRC_ReceiveConnSetupCmpl::lt_FirstValue
Attach:[18] Enter Test Step ts_RRC_ReceiveConnSetupCmpl::lt_SecondValue( 0 )
| Assignment:[26] start_CS := '00000000000000000010'B Attach:[18] Exit Test Step ts_RRC_ReceiveConnSetupCmpl::lt_SecondValue
Attach:[6] Exit Test Step ts_RRC_ReceiveConnSetupCmpl::lt_GetHFN
Attach:[5] Exit Test Step ts_RRC_ReceiveConnSetupCmpl
Attach:[6] Exit Test Step ts_RRC_ConnEst
Attach:[8] Enter Test Step ts_GMM_DetachOnSwitchOff::lt_Detach_PSonly( 0 )
| Attach:[8] Exit Test Step ts_GMM_DetachOnSwitchOff::lt_Detach_PSonly
00:01:01.140 - Primitive: RLC_AM_DATA_IND: initialDirectTransfer 00:01:01.140 - Primitive: RRC_DATA_IND: gmm:detachRequest Attach:[8] Enter Test Step ts_GMM_DetachOnSwitchOff::lt_Detach_PSonly( 0 )
| begin "car_PS_InitDirectTransfer" of type RRC_DataInd (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "rB_Id" of type SS_RB_Identity (INTEGER) [UNIVERSAL 2] matching 3 against 3 end "rB_Id" of type SS_RB_Identity begin "cN_Domain" of type SS_CN_DomainIdentity (INTEGER) [UNIVERSAL 2] matching 1 against 1 end "cN_Domain" of type SS_CN_DomainIdentity begin "start" of type START_Value (BITSTRING) [UNIVERSAL 3] matching '00000000000000000010'B against ? end "start" of type START_Value begin "msg" of type DETACHREQUESTMO (SEQUENCE) [UNIVERSAL 16] begin "skipIndicator" of type SkipIndicator (BITSTRING) [UNIVERSAL 3] matching '0000'B against '0000'B end "skipIndicator" of type SkipIndicator begin "gMMProtocolDiscriminator" of type ProtocolDiscriminator (BITSTRING) [UNIVERSAL 3] matching '1000'B against '1000'B end "gMMProtocolDiscriminator" of type ProtocolDiscriminator begin "msgType" of type MsgType (BITSTRING) [UNIVERSAL 3] matching '00000101'B against '00000101'B end "msgType" of type MsgType begin "spare4" of type B4 (BITSTRING) [UNIVERSAL 3] matching '0000'B against ? end "spare4" of type B4 begin "detachType" of type DetachType (SEQUENCE) [UNIVERSAL 16] begin "powOff" of type B1 (BITSTRING) [UNIVERSAL 3] matching '1'B against '1'B end "powOff" of type B1 begin "type" of type B3 (BITSTRING) [UNIVERSAL 3] matching '001'B against '001'B end "type" of type B3 end "detachType" of type DetachType begin "ptmsi" of type GMM_MS_IdentityPTMSI (SEQUENCE) [UNIVERSAL 16] begin "iei" of type IEI8 (BITSTRING) [UNIVERSAL 3] matching '00011000'B against '00011000'B end "iei" of type IEI8 begin "iel" of type Length (OCTETSTRING) [UNIVERSAL 4] matching '05'O against '05'O end "iel" of type Length begin "iDigit1" of type B4 (BITSTRING) [UNIVERSAL 3] matching '1111'B against '1111'B end "iDigit1" of type B4 begin "oddEvenInd" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against '0'B end "oddEvenInd" of type B1 begin "typeOfId" of type B3 (BITSTRING) [UNIVERSAL 3] matching '100'B against '100'B end "typeOfId" of type B3 begin "otherDigits" of type OCTETSTRING [UNIVERSAL 4] matching '12345678'O against '12345678'O end "otherDigits" of type OCTETSTRING end "ptmsi" of type GMM_MS_IdentityPTMSI begin "ptmsiSignature" of type PTMSI_Signature_tlv (SEQUENCE) [UNIVERSAL 16] begin "iei" of type IEI8 (BITSTRING) [UNIVERSAL 3] matching '00011001'B against '00011001'B end "iei" of type IEI8 begin "iel" of type Length (OCTETSTRING) [UNIVERSAL 4] matching '03'O against '03'O end "iel" of type Length begin "value" of type OCTETSTRING [UNIVERSAL 4] matching 'AB1234'O against 'AB1234'O end "value" of type OCTETSTRING end "ptmsiSignature" of type PTMSI_Signature_tlv end "msg" of type DETACHREQUESTMO end "car_PS_InitDirectTransfer" of type RRC_DataInd Receive event:[26] Dc ? RRC_DataInd = PDU (view PDU) Preliminary verdict:[26] (PASS) Attach:[8] Exit Test Step ts_GMM_DetachOnSwitchOff::lt_Detach_PSonly
Attach:[9] Enter Test Step ts_RRC_ConnRel_AfterSwitchOff( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[2] Enter Test Step ts_RRC_Delay( 1000 )
| StartTimer:[1] t_Dly [5000] 1000 ms Timed out Timer:t_Dly TimeOut:[2] t_Dly [5000] 1000 ms Attach:[2] Exit Test Step ts_RRC_Delay
Attach:[3] Enter Test Step ts_RRC_ConnRel_AfterSwitchOff::lt_Send_RRC_ConnectionRelease( 0 )
| Assignment:[39] tcv_N308 := 1 Assignment:[39] tcv_K := 1 00:01:02.170 - Primitive: RLC_UM_DATA_REQ 00:01:02.170 - Primitive: RLC_UM_DATA_REQ: rrcConnectionRelease Send event:[40] UM ! RLC_UM_DATA_REQ = PDU (view PDU) StartTimer:[41] t_Dly [5000] 1000 ms 00:01:02.430 - Primitive: RLC_UM_DATA_IND: rrcConnectionReleaseComplete 00:01:02.430 - Primitive: RLC_UM_DATA_IND begin "car_RRC_ConnRelCmplUM" of type RLC_UM_DATA_IND (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "integrityResult" of type IntegrityResult (CHOICE) [UNIVERSAL 31] matching [integrityUsed: i_pass] against * end "integrityResult" of type IntegrityResult begin "uM_message" of type CHOICE [UNIVERSAL 31] begin "uL_DCCH_Message" of type UL_DCCH_Message (SEQUENCE) [UNIVERSAL 16] begin "message" of type UL_DCCH_MessageType (CHOICE) [UNIVERSAL 31] begin "rrcConnectionReleaseComplete" of type RRCConnectionReleaseComplete (SEQUENCE) [UNIVERSAL 16] begin "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier (INTEGER) [UNIVERSAL 2] matching 0 against 0 end "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier end "rrcConnectionReleaseComplete" of type RRCConnectionReleaseComplete end "message" of type UL_DCCH_MessageType end "uL_DCCH_Message" of type UL_DCCH_Message end "uM_message" of type CHOICE end "car_RRC_ConnRelCmplUM" of type RLC_UM_DATA_IND CancelTimer:TSP1: [43] t_Dly [5000] 1000 ms Receive event:TSP1: [43] UM ? RLC_UM_DATA_IND = PDU (view PDU) Preliminary verdict:TSP1: [43] (PASS) Attach:[44] Enter Test Step ts_RRC_ConnRel_AfterSwitchOff::lt_RptRcvConnRel( 0 )
| StartTimer:[54] t_Dly [5000] 5000 ms 00:01:02.600 - Primitive: RLC_UM_DATA_IND: rrcConnectionReleaseComplete 00:01:02.600 - Primitive: RLC_UM_DATA_IND begin "car_RRC_ConnRelCmplUM" of type RLC_UM_DATA_IND (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "integrityResult" of type IntegrityResult (CHOICE) [UNIVERSAL 31] matching [integrityUsed: i_pass] against * end "integrityResult" of type IntegrityResult begin "uM_message" of type CHOICE [UNIVERSAL 31] begin "uL_DCCH_Message" of type UL_DCCH_Message (SEQUENCE) [UNIVERSAL 16] begin "message" of type UL_DCCH_MessageType (CHOICE) [UNIVERSAL 31] begin "rrcConnectionReleaseComplete" of type RRCConnectionReleaseComplete (SEQUENCE) [UNIVERSAL 16] begin "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier (INTEGER) [UNIVERSAL 2] matching 0 against 0 end "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier end "rrcConnectionReleaseComplete" of type RRCConnectionReleaseComplete end "message" of type UL_DCCH_MessageType end "uL_DCCH_Message" of type UL_DCCH_Message end "uM_message" of type CHOICE end "car_RRC_ConnRelCmplUM" of type RLC_UM_DATA_IND Assignment:TSP2: [57] tcv_K := 2 CancelTimer:TSP2: [57] t_Dly [5000] 5000 ms Receive event:TSP2: [57] UM ? RLC_UM_DATA_IND = PDU (view PDU) Preliminary verdict:TSP2: [57] (PASS) Attach:[44] Exit Test Step ts_RRC_ConnRel_AfterSwitchOff::lt_RptRcvConnRel
Attach:[3] Exit Test Step ts_RRC_ConnRel_AfterSwitchOff::lt_Send_RRC_ConnectionRelease
Attach:[4] Enter Test Step ts_RRC_ConnRel_AfterSwitchOff::lt_RestartCRLC_ForNextConnection( 0 )
| Attach:[7] Enter Test Step ts_CRLC_RelReconfSRB( 0 )
| Attach:[1] Enter Test Step ts_CRLC_Rel( -1 )
| 00:01:02.600 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:02.620 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 1 ]} Attach:[1] Exit Test Step ts_CRLC_Rel
Attach:[2] Enter Test Step ts_CRLC_Rel( -1 )
| 00:01:02.620 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:02.630 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 2 ]} Attach:[2] Exit Test Step ts_CRLC_Rel
Attach:[3] Enter Test Step ts_CRLC_Rel( -1 )
| 00:01:02.630 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:02.650 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 3 ]} Attach:[3] Exit Test Step ts_CRLC_Rel
Attach:[4] Enter Test Step ts_CRLC_Rel( -1 )
| 00:01:02.650 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:02.670 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 4 ]} Attach:[4] Exit Test Step ts_CRLC_Rel
Attach:[5] Enter Test Step ts_SS_RB1_ToRB4_Cfg( )
| 00:01:02.670 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:02.680 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 1 ]} 00:01:02.680 - Primitive: CRLC_Config_REQ Send event:[3] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:02.700 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[4] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 2 ]} 00:01:02.700 - Primitive: CRLC_Config_REQ Send event:[5] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:02.710 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[6] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 3 ]} 00:01:02.710 - Primitive: CRLC_Config_REQ Send event:[7] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:02.730 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[8] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 4 ]} Attach:[5] Exit Test Step ts_SS_RB1_ToRB4_Cfg
Attach:[7] Exit Test Step ts_CRLC_RelReconfSRB
Attach:[8] Enter Test Step ts_SetCellCfg( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Assignment:[2] cellConfig := cell_DCH_StandAloneSRB_NoConn Attach:[3] Enter Test Step ts_SaveCellInfo( 0 )
| Assignment:[2] tcv_CellInfoA := (view Assignment) Attach:[3] Exit Test Step ts_SaveCellInfo
Attach:[8] Exit Test Step ts_SetCellCfg
Attach:[4] Exit Test Step ts_RRC_ConnRel_AfterSwitchOff::lt_RestartCRLC_ForNextConnection
Attach:[5] Enter Test Step ts_SS_ResetSecurityKey( )
| Assignment:[1] tcv_CellIndInfo := (view Assignment) Assignment:[3] cipheringAlgorithmCapability := '0000000000000011'B Attach:[5] Exit Test Step ts_SS_ResetSecurityKey
Attach:[9] Exit Test Step ts_RRC_ConnRel_AfterSwitchOff
Attach:[9] Exit Test Step ts_GMM_DetachOnSwitchOff
Attach:[10] Enter Test Step tc_12_4_1_2::lt_TestBody( )
| Assignment:[12] tcv_TestBody := GcTRUE Preliminary verdict:[12] (PASS) Attach:[13] Enter Test Step ts_MMI_UE_SwitchOnTriggerGMM_Attach( )
| Attach:[1] Enter Test Step ts_GMM_SwitchOrPwrOn( )
| Attach:[2] Enter Test Step ts_MMI_UE_SwitchOn( )
| 00:01:02.730 - Primitive: MMI_CmdReq Send event:[2] Ut ! MMI_CmdReq = PDU: { cmd: "Please switch on the UE" } 00:01:06.130 - Primitive: MMI_CmdCnf begin "ca_MMI_CmdCnf" of type MMI_CmdCnf (SEQUENCE) [UNIVERSAL 16] begin "result" of type BOOLEAN [UNIVERSAL 1] matching GcTRUE against GcTRUE end "result" of type BOOLEAN end "ca_MMI_CmdCnf" of type MMI_CmdCnf Receive event:[3] Ut ? MMI_CmdCnf = PDU: { result: GcTRUE , resultString: OMIT} Assignment:[4] tcv_UE_SwitchedOn := GcTRUE Attach:[2] Exit Test Step ts_MMI_UE_SwitchOn
Attach:[1] Exit Test Step ts_GMM_SwitchOrPwrOn
Attach:[4] Enter Test Step ts_NAS_Delay( 5000 )
| StartTimer:[1] t_Dly [5000] 5000 ms Timed out Timer:t_Dly TimeOut:[2] t_Dly [5000] 5000 ms Attach:[4] Exit Test Step ts_NAS_Delay
Attach:[5] Enter Test Step ts_AT_TriggerGMM_Attach( )
| 00:01:11.150 - Primitive: AT_CmdReq Send event:[1] Ut ! AT_CmdReq = PDU: { cmd: "AT+CGATT=1<CR>" , sMS_BlockMode: OMIT} 00:01:15.210 - Primitive: AT_CmdCnf begin "ca_AT_CmdCnf" of type AT_CmdCnf (SEQUENCE) [UNIVERSAL 16] begin "resultString" of type IA5String [UNIVERSAL 22] matching "<CR><LF>OK<CR><LF>" against "<CR><LF>OK<CR><LF>" IF PRESENT end "resultString" of type IA5String end "ca_AT_CmdCnf" of type AT_CmdCnf Receive event:[2] Ut ? AT_CmdCnf = PDU (view PDU) Attach:[5] Exit Test Step ts_AT_TriggerGMM_Attach
Attach:[13] Exit Test Step ts_MMI_UE_SwitchOnTriggerGMM_Attach
Attach:[14] Enter Test Step ts_RRC_ConnEst( 0 )
| Attach:[1] Enter Test Step ts_SS_PrepareCellRRC_ConnEst( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[1] Exit Test Step ts_SS_PrepareCellRRC_ConnEst
Attach:[2] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[2] Exit Test Step ts_SetTmpCellInfo
Attach:[3] Enter Test Step ts_RRC_ConnEst::lt_RcvConnReq( 0 )
| 00:01:33.960 - Primitive: RLC_TR_DATA_IND: rrcConnectionRequest 00:01:33.960 - Primitive: RLC_TR_DATA_IND begin "car_RRC_ConnReq" of type RLC_TR_DATA_IND (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "tM_message" of type CHOICE [UNIVERSAL 31] begin "uL_CCCH_Message" of type UL_CCCH_Message (SEQUENCE) [UNIVERSAL 16] begin "message" of type UL_CCCH_MessageType (CHOICE) [UNIVERSAL 31] begin "rrcConnectionRequest" of type RRCConnectionRequest (SEQUENCE) [UNIVERSAL 16] begin "initialUE_Identity" of type InitialUE_Identity (CHOICE) [UNIVERSAL 31] begin InitialUE_Identity (CHOICE) [UNIVERSAL 31] end InitialUE_Identity begin InitialUE_Identity (CHOICE) [UNIVERSAL 31] begin "tmsi_and_LAI" of type TMSI_and_LAI_GSM_MAP (SEQUENCE) [UNIVERSAL 16] matching { tmsi: '00010001001000100011001101000100'B , lai: { plmn_Identity: { mcc: [ 0 , 0 , 1 ] , mnc: [ 0 , 1 ] } , lac: '0000000000000001'B } } against ? end "tmsi_and_LAI" of type TMSI_and_LAI_GSM_MAP end InitialUE_Identity matching [tmsi_and_LAI: { tmsi: '00010001001000100011001101000100'B , lai: { plmn_Identity: { mcc: [ 0 , 0 , 1 ] , mnc: [ 0 , 1 ] } , lac: '0000000000000001'B } } ] against ([imsi: ?], [tmsi_and_LAI: ?], [p_TMSI_and_RAI: ?], [imei: ?]) end "initialUE_Identity" of type InitialUE_Identity begin "establishmentCause" of type EstablishmentCause (ENUMERATED) [UNIVERSAL 10] matching registration against registration end "establishmentCause" of type EstablishmentCause begin "protocolErrorIndicator" of type ProtocolErrorIndicator (ENUMERATED) [UNIVERSAL 10] matching noError against noError end "protocolErrorIndicator" of type ProtocolErrorIndicator end "rrcConnectionRequest" of type RRCConnectionRequest end "message" of type UL_CCCH_MessageType end "uL_CCCH_Message" of type UL_CCCH_Message end "tM_message" of type CHOICE end "car_RRC_ConnReq" of type RLC_TR_DATA_IND Assignment:[7] tcv_InitialUE_Id := (view Assignment) Receive event:[7] TM ? RLC_TR_DATA_IND = PDU (view PDU) Attach:[3] Exit Test Step ts_RRC_ConnEst::lt_RcvConnReq
Attach:[4] Enter Test Step ts_RRC_ConnEst::lt_Send_ConnSetUp( 0 )
| 00:01:33.960 - Primitive: RLC_UM_DATA_REQ 00:01:33.960 - Primitive: RLC_UM_DATA_REQ: rrcConnectionSetup Send event:[31] UM ! RLC_UM_DATA_REQ = PDU (view PDU) Attach:[33] Enter Test Step ts_SetCellCfg( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Assignment:[2] cellConfig := cell_DCH_StandAloneSRB Attach:[3] Enter Test Step ts_SaveCellInfo( 0 )
| Assignment:[2] tcv_CellInfoA := (view Assignment) Attach:[3] Exit Test Step ts_SaveCellInfo
Attach:[33] Exit Test Step ts_SetCellCfg
Attach:[4] Exit Test Step ts_RRC_ConnEst::lt_Send_ConnSetUp
Attach:[5] Enter Test Step ts_RRC_ReceiveConnSetupCmpl( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
StartTimer:[3] t_WaitMS [13500] 13500 ms 00:01:34.450 - Primitive: RLC_AM_DATA_IND: rrcConnectionSetupComplete 00:01:34.450 - Primitive: RLC_AM_DATA_IND begin "car_RRC_ConnSetupCmpl" of type RLC_AM_DATA_IND (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "integrityResult" of type IntegrityResult (CHOICE) [UNIVERSAL 31] matching [integrityUsed: i_pass] against ? end "integrityResult" of type IntegrityResult begin "aM_message" of type CHOICE [UNIVERSAL 31] begin "uL_DCCH_Message" of type UL_DCCH_Message (SEQUENCE) [UNIVERSAL 16] begin "message" of type UL_DCCH_MessageType (CHOICE) [UNIVERSAL 31] begin "rrcConnectionSetupComplete" of type RRCConnectionSetupComplete (SEQUENCE) [UNIVERSAL 16] begin "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier (INTEGER) [UNIVERSAL 2] matching 0 against 0 end "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier begin "startList" of type STARTList (SEQUENCEOF) [UNIVERSAL 28] matching [ { cn_DomainIdentity: ps_domain, start_Value: '00000000000000000010'B } , { cn_DomainIdentity: cs_domain, start_Value: '00000000000000000010'B } ] against ? end "startList" of type STARTList begin "ue_RadioAccessCapability" of type UE_RadioAccessCapability (SEQUENCE) [UNIVERSAL 16] matching { accessStratumReleaseIndicator: r99, pdcp_Capability: { losslessSRNS_RelocationSupport: GcFALSE , supportForRfc2507: [notSupported: NULL]} , rlc_Capability: { totalRLC_AM_BufferSize: kb50, maximumRLC_WindowSize: mws2047, maximumAM_EntityNumber: am6} , transportChannelCapability: { dl_TransChCapability: { maxNoBitsReceived: b8960, maxConvCodeBitsReceived: b1280, turboDecodingSupport: [supported: b8960], maxSimultaneousTransChs: e8, maxSimultaneousCCTrCH_Count: 1 , maxReceivedTransportBlocks: tb32, maxNumberOfTFC: tfc128, maxNumberOfTF: tf64} , ul_TransChCapability: { maxNoBitsTransmitted: b3840, maxConvCodeBitsTransmitted: b1280, turboEncodingSupport: [supported: b3840], maxSimultaneousTransChs: e8, modeSpecificInfo: [fdd: NULL], maxTransmittedBlocks: tb32, maxNumberOfTFC: tfc64, maxNumberOfTF: tf32} } , rf_Capability: { fddRF_Capability: { ue_PowerClass: 4 , txRxFrequencySeparation: mhz190} , tddRF_Capability: OMIT} , physicalChannelCapability: { fddPhysChCapability: { downlinkPhysChCapability: { maxNoDPCH_PDSCH_Codes: 1 , maxNoPhysChBitsReceived: b9600, supportForSF_512: GcFALSE , supportOfPDSCH: GcFALSE , simultaneousSCCPCH_DPCH_Reception: [notSupported: NULL]} , uplinkPhysChCapability: { maxNoDPDCH_BitsTransmitted: b4800, supportOfPCPCH: GcFALSE } } , tddPhysChCapability: OMIT} , ue_MultiModeRAT_Capability: { multiRAT_CapabilityList: { supportOfGSM: GcFALSE , supportOfMulticarrier: GcFALSE } , multiModeCapability: fdd} , securityCapability: { cipheringAlgorithmCap: '0000000000000011'B , integrityProtectionAlgorithmCap: '0000000000000010'B } , ue_positioning_Capability: { standaloneLocMethodsSupported: GcFALSE , ue_BasedOTDOA_Supported: GcFALSE , networkAssistedGPS_Supported: noNetworkAssistedGPS, supportForUE_GPS_TimingOfCellFrames: GcFALSE , supportForIPDL: GcFALSE } , measurementCapability: { downlinkCompressedMode: { fdd_Measurements: GcTRUE , tdd_Measurements: OMIT, gsm_Measurements: { gsm900: GcTRUE , dcs1800: GcTRUE , gsm1900: GcTRUE } , multiCarrierMeasurements: GcFALSE } , uplinkCompressedMode: { fdd_Measurements: GcTRUE , tdd_Measurements: OMIT, gsm_Measurements: { gsm900: GcTRUE , dcs1800: GcTRUE , gsm1900: GcTRUE } , multiCarrierMeasurements: GcFALSE } } } against * end "ue_RadioAccessCapability" of type UE_RadioAccessCapability end "rrcConnectionSetupComplete" of type RRCConnectionSetupComplete end "message" of type UL_DCCH_MessageType end "uL_DCCH_Message" of type UL_DCCH_Message end "aM_message" of type CHOICE end "car_RRC_ConnSetupCmpl" of type RLC_AM_DATA_IND Assignment:TSP1: [5] tcv_StartList := (view Assignment) Assignment:TSP1: [5] cipheringAlgorithmCapability := '0000000000000011'B CancelTimer:TSP1: [5] t_WaitMS [13500] 13500 ms Receive event:TSP1: [5] AM ? RLC_AM_DATA_IND = PDU (view PDU) Preliminary verdict:TSP1: [5] (PASS) Attach:[6] Enter Test Step ts_RRC_ReceiveConnSetupCmpl::lt_GetHFN( 0 )
| Assignment:[13] tcv_Count := 2 Attach:[17] Enter Test Step ts_RRC_ReceiveConnSetupCmpl::lt_FirstValue( 0 )
| Assignment:[23] start_PS := '00000000000000000010'B Attach:[17] Exit Test Step ts_RRC_ReceiveConnSetupCmpl::lt_FirstValue
Attach:[18] Enter Test Step ts_RRC_ReceiveConnSetupCmpl::lt_SecondValue( 0 )
| Assignment:[26] start_CS := '00000000000000000010'B Attach:[18] Exit Test Step ts_RRC_ReceiveConnSetupCmpl::lt_SecondValue
Attach:[6] Exit Test Step ts_RRC_ReceiveConnSetupCmpl::lt_GetHFN
Attach:[5] Exit Test Step ts_RRC_ReceiveConnSetupCmpl
Attach:[14] Exit Test Step ts_RRC_ConnEst
Attach:[15] Enter Test Step tc_12_4_1_2::lt_Attach_Steps_4To5( )
| Attach:[15] Exit Test Step tc_12_4_1_2::lt_Attach_Steps_4To5
00:01:34.460 - Primitive: RLC_AM_DATA_IND: initialDirectTransfer 00:01:34.460 - Primitive: RRC_DATA_IND: gmm:attachRequest Attach:[15] Enter Test Step tc_12_4_1_2::lt_Attach_Steps_4To5( )
| begin "car_PS_InitDirectTransfer" of type RRC_DataInd (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "rB_Id" of type SS_RB_Identity (INTEGER) [UNIVERSAL 2] matching 3 against 3 end "rB_Id" of type SS_RB_Identity begin "cN_Domain" of type SS_CN_DomainIdentity (INTEGER) [UNIVERSAL 2] matching 1 against 1 end "cN_Domain" of type SS_CN_DomainIdentity begin "start" of type START_Value (BITSTRING) [UNIVERSAL 3] matching '00000000000000000010'B against ? end "start" of type START_Value begin "msg" of type ATTACHREQUEST (SEQUENCE) [UNIVERSAL 16] begin "skipIndicator" of type SkipIndicator (BITSTRING) [UNIVERSAL 3] matching '0000'B against '0000'B end "skipIndicator" of type SkipIndicator begin "gMMProtocolDiscriminator" of type ProtocolDiscriminator (BITSTRING) [UNIVERSAL 3] matching '1000'B against '1000'B end "gMMProtocolDiscriminator" of type ProtocolDiscriminator begin "msgType" of type MsgType (BITSTRING) [UNIVERSAL 3] matching '00000001'B against '00000001'B end "msgType" of type MsgType begin "msNetworkCap" of type MS_NetworkCap_lv (SEQUENCE) [UNIVERSAL 16] matching { iel: '02'O , value: 'E540'O } against ? end "msNetworkCap" of type MS_NetworkCap_lv begin "gprsCiphKeySeqNo" of type CiphKeySeqNum (SEQUENCE) [UNIVERSAL 16] begin "spare1" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against '0'B end "spare1" of type B1 begin "keySeq" of type KeySeq (BITSTRING) [UNIVERSAL 3] matching '000'B against '000'B end "keySeq" of type KeySeq end "gprsCiphKeySeqNo" of type CiphKeySeqNum begin "attachType" of type AttachType (SEQUENCE) [UNIVERSAL 16] begin "for" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against '0'B end "for" of type B1 begin "type" of type B3 (BITSTRING) [UNIVERSAL 3] matching '001'B against '001'B end "type" of type B3 end "attachType" of type AttachType begin "drxParameter" of type DRXparamter (SEQUENCE) [UNIVERSAL 16] matching { splitPGcycleCode: '00000111'B , cnDRXcoef: '0000'B , splitOnCCCH: '0'B , nonDRXtimer: '100'B } against ? end "drxParameter" of type DRXparamter begin "ptmsiORimsi" of type MS_Identity_lv (SEQUENCE) [UNIVERSAL 16] begin "iel" of type Length (OCTETSTRING) [UNIVERSAL 4] matching '05'O against '05'O end "iel" of type Length begin "iDigit1" of type B4 (BITSTRING) [UNIVERSAL 3] matching '1111'B against '1111'B end "iDigit1" of type B4 begin "oddEvenInd" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against '0'B end "oddEvenInd" of type B1 begin "typeOfId" of type B3 (BITSTRING) [UNIVERSAL 3] matching '100'B against '100'B end "typeOfId" of type B3 begin "otherDigits" of type OCTETSTRING [UNIVERSAL 4] matching '12345678'O against '12345678'O end "otherDigits" of type OCTETSTRING end "ptmsiORimsi" of type MS_Identity_lv begin "oldRAI" of type RAI_v (SEQUENCE) [UNIVERSAL 16] begin "plmn" of type OCTETSTRING [UNIVERSAL 4] matching '00F110'O against '00F110'O end "plmn" of type OCTETSTRING begin "lac" of type OCTETSTRING [UNIVERSAL 4] matching '0001'O against '0001'O end "lac" of type OCTETSTRING begin "rac" of type OCTETSTRING [UNIVERSAL 4] matching '05'O against '05'O end "rac" of type OCTETSTRING end "oldRAI" of type RAI_v begin "msRadioAccessCap" of type MSRadioAccessCap_lv (SEQUENCE) [UNIVERSAL 16] matching { iel: '0B'O , value: '15F38233542A332644A198'O } against ? end "msRadioAccessCap" of type MSRadioAccessCap_lv begin "readyTimer" of type GPRS_Timer (SEQUENCE) [UNIVERSAL 16] begin "iei" of type IEI8 (BITSTRING) [UNIVERSAL 3] matching '00010111'B against '00010111'B end "iei" of type IEI8 begin "unit" of type B3 (BITSTRING) [UNIVERSAL 3] matching '000'B against ? end "unit" of type B3 begin "value" of type B5 (BITSTRING) [UNIVERSAL 3] matching '10110'B against ? end "value" of type B5 end "readyTimer" of type GPRS_Timer end "msg" of type ATTACHREQUEST end "car_PS_InitDirectTransfer" of type RRC_DataInd Assignment:[27] tcv_Start := '00000000000000000010'B Receive event:[27] Dc ? RRC_DataInd = PDU (view PDU) Attach:[28] Enter Test Step ts_SS_SecurityDownloadStart( ps_domain )
| Assignment:[4] start_PS := '00000000000000000010'B Attach:[28] Exit Test Step ts_SS_SecurityDownloadStart
Attach:[29] Enter Test Step ts_GMM_AuthenticateAndStartIntegrityProtection( 0 )
| Attach:[1] Enter Test Step ts_GMM_Authentication( 0 )
| Attach:[1] Enter Test Step ts_GMM_AuthenticationInit( )
| Attach:[1] Enter Test Step ts_GMM_AuthenticationInit::lt_IncrementCiphKeySeqNum( )
| Assignment:[6] tcv_PS_KeySeq := '001'B Attach:[1] Exit Test Step ts_GMM_AuthenticationInit::lt_IncrementCiphKeySeqNum
Attach:[2] Enter Test Step ts_GMM_AuthenticationInit::lt_AuthCalcAUTN( )
| Assignment:[19] tcv_AuthXDOUT := (view Assignment) Assignment:[20] tcv_AuthCDOUT := '0000000000000000000000000000000000000000000000000000000000000000'B Assignment:[21] tcv_AuthXDOUT_Half := '0101010101000100011101110110011000010001000000000011001100100010'B Assignment:[22] tcv_AuthAK := '011001100001000100000000001100110010001011011101'B Assignment:[23] tcv_AuthAUTN_1 := '011001100001000100000000001100110010001011011101'B Assignment:[24] tcv_AuthMAC := '0101010101000100011101110110011000010001000000000011001100100010'B Assignment:[25] tcv_AuthAUTN_2 := (view Assignment) Assignment:[26] tcv_AuthAUTN := (view Assignment) Attach:[2] Exit Test Step ts_GMM_AuthenticationInit::lt_AuthCalcAUTN
Attach:[3] Enter Test Step ts_GMM_AuthenticationInit::lt_AuthCalcUMTS_Others( )
| Assignment:[27] tcv_PS_AuthIK := (view Assignment) Assignment:[28] tcv_PS_AuthCK := (view Assignment) Assignment:[29] tcv_AuthXRES := (view Assignment) Attach:[3] Exit Test Step ts_GMM_AuthenticationInit::lt_AuthCalcUMTS_Others
Attach:[4] Enter Test Step ts_GMM_AuthenticationInit::lt_AuthCalcKcGSM( )
| Assignment:[30] tcv_AuthCK_1 := '0100010001110111011001100001000100000000001100110010001011011101'B Assignment:[31] tcv_AuthCK_2 := '1100110011111111111011101001100110001000101110111010101001010101'B Assignment:[32] tcv_AuthIK_1 := '0111011101100110000100010000000000110011001000101101110111001100'B Assignment:[33] tcv_AuthIK_2 := '1111111111101110100110011000100010111011101010100101010101000100'B Assignment:[34] tcv_AuthCK_XOR := '1000100010001000100010001000100010001000100010001000100010001000'B Assignment:[35] tcv_AuthIK_XOR := '1000100010001000100010001000100010001000100010001000100010001000'B Assignment:[36] tcv_AuthKcGSM := '0000000000000000000000000000000000000000000000000000000000000000'B Attach:[4] Exit Test Step ts_GMM_AuthenticationInit::lt_AuthCalcKcGSM
Attach:[1] Exit Test Step ts_GMM_AuthenticationInit
00:01:34.480 - Primitive: RRC_DATA_REQ: gmm:authenticationAndCipheringRequest 00:01:34.480 - Primitive: RLC_AM_DATA_REQ:downlinkDirectTransfer Send event:[2] Dc ! RRC_DataReq = PDU (view PDU) 00:01:34.940 - Primitive: RLC_AM_DATA_IND: uplinkDirectTransfer 00:01:34.940 - Primitive: RRC_DATA_IND: gmm:authenticationAndCipheringResponse begin "car_PS_UplinkDirectTransfer" of type RRC_DataInd (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "rB_Id" of type SS_RB_Identity (INTEGER) [UNIVERSAL 2] matching 3 against 3 end "rB_Id" of type SS_RB_Identity begin "cN_Domain" of type SS_CN_DomainIdentity (INTEGER) [UNIVERSAL 2] matching 1 against 1 end "cN_Domain" of type SS_CN_DomainIdentity begin "msg" of type AUTHENTICATIONANDCIPHERINGRESPONSE (SEQUENCE) [UNIVERSAL 16] begin "skipIndicator" of type SkipIndicator (BITSTRING) [UNIVERSAL 3] matching '0000'B against '0000'B end "skipIndicator" of type SkipIndicator begin "gMMProtocolDiscriminator" of type ProtocolDiscriminator (BITSTRING) [UNIVERSAL 3] matching '1000'B against '1000'B end "gMMProtocolDiscriminator" of type ProtocolDiscriminator begin "msgType" of type MsgType (BITSTRING) [UNIVERSAL 3] matching '00010011'B against '00010011'B end "msgType" of type MsgType begin "spare4" of type B4 (BITSTRING) [UNIVERSAL 3] matching '0000'B against '0000'B end "spare4" of type B4 begin "acRefNo" of type AC_ReferenceNumber (SEQUENCE) [UNIVERSAL 16] matching { value: '0011'B } against ? end "acRefNo" of type AC_ReferenceNumber begin "authRsp" of type AuthRsp_tv (SEQUENCE) [UNIVERSAL 16] begin "iei" of type IEI8 (BITSTRING) [UNIVERSAL 3] matching '00100010'B against '00100010'B end "iei" of type IEI8 begin "value" of type BITSTRING [UNIVERSAL 3] matching '01010101010001000111011101100110'B against ? end "value" of type BITSTRING end "authRsp" of type AuthRsp_tv begin "authRspExt" of type AuthRspExt (SEQUENCE) [UNIVERSAL 16] begin "iei" of type IEI8 (BITSTRING) [UNIVERSAL 3] matching '00101001'B against '00101001'B end "iei" of type IEI8 begin "iel" of type Length (OCTETSTRING) [UNIVERSAL 4] matching '04'O against ? end "iel" of type Length begin "rES" of type BITSTRING [UNIVERSAL 3] matching '00010001000000000011001100100010'B against ? end "rES" of type BITSTRING end "authRspExt" of type AuthRspExt end "msg" of type AUTHENTICATIONANDCIPHERINGRESPONSE end "car_PS_UplinkDirectTransfer" of type RRC_DataInd Assignment:[3] tcv_TmpAuthAndCiphRspPDU (view PDU) Assignment:[3] tcv_AuthRsp := '01010101010001000111011101100110'B Assignment:[3] tcv_AuthRspExt := { iei: '00101001'B , iel: '04'O , rES: '00010001000000000011001100100010'B } Receive event:[3] Dc ? RRC_DataInd = PDU (view PDU) Assignment:[4] tcv_Res := GcTRUE Preliminary verdict:TSP1: [6] (PASS) Attach:[1] Exit Test Step ts_GMM_Authentication
Attach:[2] Enter Test Step ts_RRC_Security( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[2] Enter Test Step ts_RRC_Security::lt_RRC_InitVariables( 0 )
| Attach:[53] Enter Test Step ts_RRC_Security::lt_InitCipherMode( 0 )
| Assignment:[82] cs_cipheringStarted := GcFALSE Assignment:[82] ps_cipheringStarted := GcFALSE Assignment:[84] cipheringAlgorithmCapability := '0000000000000011'B Attach:[53] Exit Test Step ts_RRC_Security::lt_InitCipherMode
Attach:[54] Enter Test Step ts_RRC_Security::lt_InitIntegrity( 0 )
| Assignment:[87] recentSecureDomain := ps_domain Assignment:[92] dL_Integrity := (view Assignment) Assignment:[92] integrityStarted := GcTRUE Assignment:[92] dl_IntegrityCheckInfo := (view Assignment) Assignment:[92] tcv_Int_ModifyFlag := GcFALSE Attach:[54] Exit Test Step ts_RRC_Security::lt_InitIntegrity
Attach:[55] Enter Test Step ts_InitSystemSpecificCap( )
| Assignment:[11] tcv_UE_SystemSpecificCap := 0 Attach:[55] Exit Test Step ts_InitSystemSpecificCap
Attach:[56] Enter Test Step ts_SaveCellInfo( 0 )
| Assignment:[2] tcv_CellInfoA := (view Assignment) Attach:[56] Exit Test Step ts_SaveCellInfo
Assignment:[58] tcv_HFN := '00000000000000000000'B Assignment:[62] start_PS := '00000000000000000000'B Attach:[2] Exit Test Step ts_RRC_Security::lt_RRC_InitVariables
Attach:[3] Enter Test Step ts_SS_DownloadSecurityKey( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[15] Enter Test Step ts_SS_DownloadSecurityKey::lt_DownloadKeyCRLC( '00000000000000000000'B )
| 00:01:34.930 - Primitive: CRLC_SecurityMode_Config_REQ 00:01:34.930 - Primitive: CRLC_SecurityMode_Config_REQ Send event:[21] CRLC ! CRLC_SecurityMode_Config_REQ = PDU (view PDU) 00:01:34.950 - Primitive: CRLC_SecurityMode_Config_CNF begin "ca_CRLC_SecurityModeCfgCnf" of type CRLC_SecurityMode_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER end "ca_CRLC_SecurityModeCfgCnf" of type CRLC_SecurityMode_Config_CNF Receive event:[22] CRLC ? CRLC_SecurityMode_Config_CNF = PDU: { cellId: -1 } Attach:[15] Exit Test Step ts_SS_DownloadSecurityKey::lt_DownloadKeyCRLC
Attach:[3] Exit Test Step ts_SS_DownloadSecurityKey
Attach:[4] Enter Test Step ts_RRC_Security::lt_ActivateSecurity_DL_SS( 0 )
| Attach:[14] Enter Test Step ts_RRC_Security::lt_InitialiseRRC_MSN( 0 )
| Attach:[25] Enter Test Step ts_SetDL_RRC_MessageSN( 0 )
| 00:01:34.950 - Primitive: CRLC_SetRRC_MessageSN_REQ Send event:[1] CRLC ! CRLC_SetRRC_MessageSN_REQ = PDU (view PDU) 00:01:34.960 - Primitive: CRLC_SetRRC_MessageSN_CNF begin "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF Receive event:[2] CRLC ? CRLC_SetRRC_MessageSN_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: 0 ]} 00:01:34.960 - Primitive: CRLC_SetRRC_MessageSN_REQ Send event:[3] CRLC ! CRLC_SetRRC_MessageSN_REQ = PDU (view PDU) 00:01:34.980 - Primitive: CRLC_SetRRC_MessageSN_CNF begin "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF Receive event:[4] CRLC ? CRLC_SetRRC_MessageSN_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 1 ]} 00:01:34.980 - Primitive: CRLC_SetRRC_MessageSN_REQ Send event:[5] CRLC ! CRLC_SetRRC_MessageSN_REQ = PDU (view PDU) 00:01:34.990 - Primitive: CRLC_SetRRC_MessageSN_CNF begin "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF Receive event:[6] CRLC ? CRLC_SetRRC_MessageSN_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 2 ]} 00:01:34.990 - Primitive: CRLC_SetRRC_MessageSN_REQ Send event:[7] CRLC ! CRLC_SetRRC_MessageSN_REQ = PDU (view PDU) 00:01:35.010 - Primitive: CRLC_SetRRC_MessageSN_CNF begin "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF Receive event:[8] CRLC ? CRLC_SetRRC_MessageSN_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 3 ]} 00:01:35.010 - Primitive: CRLC_SetRRC_MessageSN_REQ Send event:[9] CRLC ! CRLC_SetRRC_MessageSN_REQ = PDU (view PDU) 00:01:35.030 - Primitive: CRLC_SetRRC_MessageSN_CNF begin "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF Receive event:[10] CRLC ? CRLC_SetRRC_MessageSN_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 4 ]} Attach:[25] Exit Test Step ts_SetDL_RRC_MessageSN
Attach:[14] Exit Test Step ts_RRC_Security::lt_InitialiseRRC_MSN
Attach:[15] Enter Test Step ts_CRLC_DL_Integrity( { integrityProtectionM ...
| (view Test Step parameters) 00:01:35.030 - Primitive: CRLC_Integrity_Activate_REQ 00:01:35.030 - Primitive: CRLC_Integrity_Activate_REQ Send event:[1] CRLC ! CRLC_Integrity_Activate_REQ = PDU (view PDU) 00:01:35.040 - Primitive: CRLC_Integrity_Activate_CNF begin "ca_CRLC_IntegrityActivateCnf" of type CRLC_Integrity_Activate_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER end "ca_CRLC_IntegrityActivateCnf" of type CRLC_Integrity_Activate_CNF Receive event:[2] CRLC ? CRLC_Integrity_Activate_CNF = PDU: { cellId: -1 } Attach:[15] Exit Test Step ts_CRLC_DL_Integrity
Attach:[4] Exit Test Step ts_RRC_Security::lt_ActivateSecurity_DL_SS
Attach:[5] Enter Test Step ts_RRC_Security::lt_RB2_UL_IntegrityActivate( 0 )
| Attach:[13] Enter Test Step ts_RB2_UL_IntegrityActivate( 0 )
| 00:01:35.040 - Primitive: CRLC_Integrity_Activate_REQ 00:01:35.040 - Primitive: CRLC_Integrity_Activate_REQ Send event:[1] CRLC ! CRLC_Integrity_Activate_REQ = PDU (view PDU) 00:01:35.060 - Primitive: CRLC_Integrity_Activate_CNF begin "ca_CRLC_IntegrityActivateCnf" of type CRLC_Integrity_Activate_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER end "ca_CRLC_IntegrityActivateCnf" of type CRLC_Integrity_Activate_CNF Receive event:[2] CRLC ? CRLC_Integrity_Activate_CNF = PDU: { cellId: -1 } Attach:[13] Exit Test Step ts_RB2_UL_IntegrityActivate
Attach:[5] Exit Test Step ts_RRC_Security::lt_RB2_UL_IntegrityActivate
Attach:[6] Enter Test Step ts_RRC_Security::lt_StartSecurity_UE( 0 )
| Attach:[27] Enter Test Step ts_RRC_Security::lt_SendSecurityModeCommand( 0 )
| 00:01:35.060 - Primitive: RLC_AM_DATA_REQ 00:01:35.060 - Primitive: RLC_AM_DATA_REQ: securityModeCommand Send event:[52] AM ! RLC_AM_DATA_REQ = PDU (view PDU) Attach:[27] Exit Test Step ts_RRC_Security::lt_SendSecurityModeCommand
00:01:35.320 - Primitive: RLC_AM_DATA_IND: securityModeComplete 00:01:35.320 - Primitive: RLC_AM_DATA_IND begin "car_RRC_SecModeCmpl" of type RLC_AM_DATA_IND (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "integrityResult" of type IntegrityResult (CHOICE) [UNIVERSAL 31] matching [integrityUsed: i_pass] against * end "integrityResult" of type IntegrityResult begin "aM_message" of type CHOICE [UNIVERSAL 31] begin "uL_DCCH_Message" of type UL_DCCH_Message (SEQUENCE) [UNIVERSAL 16] begin "integrityCheckInfo" of type IntegrityCheckInfo (SEQUENCE) [UNIVERSAL 16] matching { messageAuthenticationCode: '10001011001000110111110011100010'B , rrc_MessageSequenceNumber: 1 } against * end "integrityCheckInfo" of type IntegrityCheckInfo begin "message" of type UL_DCCH_MessageType (CHOICE) [UNIVERSAL 31] begin "securityModeComplete" of type SecurityModeComplete (SEQUENCE) [UNIVERSAL 16] begin "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier (INTEGER) [UNIVERSAL 2] matching 0 against 0 end "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier begin "ul_IntegProtActivationInfo" of type IntegrityProtActivationInfo (SEQUENCE) [UNIVERSAL 16] matching { rrc_MessageSequenceNumberList: [ 0 , 0 , 0 , 0 , 0 ] } against * end "ul_IntegProtActivationInfo" of type IntegrityProtActivationInfo end "securityModeComplete" of type SecurityModeComplete end "message" of type UL_DCCH_MessageType end "uL_DCCH_Message" of type UL_DCCH_Message end "aM_message" of type CHOICE end "car_RRC_SecModeCmpl" of type RLC_AM_DATA_IND Assignment:TSP2: [34] uL_Integrity := { rrc_MessageSequenceNumberList: [ 0 , 0 , 0 , 0 , 0 ] } Receive event:TSP2: [34] AM ? RLC_AM_DATA_IND = PDU (view PDU) Preliminary verdict:TSP2: [34] (PASS) Attach:[35] Enter Test Step ts_CRLC_UL_Integrity( { rrc_MessageSequenceNumberList: [ 0 , 0 , 0 , 0 , 0 ] } )
| 00:01:35.320 - Primitive: CRLC_Integrity_Activate_REQ 00:01:35.320 - Primitive: CRLC_Integrity_Activate_REQ Send event:[1] CRLC ! CRLC_Integrity_Activate_REQ = PDU (view PDU) 00:01:35.340 - Primitive: CRLC_Integrity_Activate_CNF begin "ca_CRLC_IntegrityActivateCnf" of type CRLC_Integrity_Activate_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER end "ca_CRLC_IntegrityActivateCnf" of type CRLC_Integrity_Activate_CNF Receive event:[2] CRLC ? CRLC_Integrity_Activate_CNF = PDU: { cellId: -1 } Attach:[35] Exit Test Step ts_CRLC_UL_Integrity
Attach:[6] Exit Test Step ts_RRC_Security::lt_StartSecurity_UE
Attach:[2] Exit Test Step ts_RRC_Security
Attach:[29] Exit Test Step ts_GMM_AuthenticateAndStartIntegrityProtection
00:01:35.340 - Primitive: RRC_DATA_REQ: gmm:attachAccept 00:01:35.340 - Primitive: RLC_AM_DATA_REQ:downlinkDirectTransfer Send event:[30] Dc ! RRC_DataReq = PDU (view PDU) Attach:[31] Enter Test Step ts_RRC_ConnRel( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[2] Enter Test Step ts_RRC_Delay( 1000 )
| StartTimer:[1] t_Dly [5000] 1000 ms Timed out Timer:t_Dly TimeOut:[2] t_Dly [5000] 1000 ms Attach:[2] Exit Test Step ts_RRC_Delay
Attach:[3] Enter Test Step ts_RRC_ConnRel::lt_Send_RRC_ConnectionRelease( 0 )
| Assignment:[39] tcv_N308 := 1 Assignment:[39] tcv_K := 1 00:01:36.340 - Primitive: RLC_UM_DATA_REQ 00:01:36.340 - Primitive: RLC_UM_DATA_REQ: rrcConnectionRelease Send event:[40] UM ! RLC_UM_DATA_REQ = PDU (view PDU) 00:01:36.600 - Primitive: RLC_UM_DATA_IND: rrcConnectionReleaseComplete 00:01:36.600 - Primitive: RLC_UM_DATA_IND begin "car_RRC_ConnRelCmplUM" of type RLC_UM_DATA_IND (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "integrityResult" of type IntegrityResult (CHOICE) [UNIVERSAL 31] matching [integrityUsed: i_pass] against * end "integrityResult" of type IntegrityResult begin "uM_message" of type CHOICE [UNIVERSAL 31] begin "uL_DCCH_Message" of type UL_DCCH_Message (SEQUENCE) [UNIVERSAL 16] begin "integrityCheckInfo" of type IntegrityCheckInfo (SEQUENCE) [UNIVERSAL 16] matching { messageAuthenticationCode: '11110111111000101100001011001110'B , rrc_MessageSequenceNumber: 1 } against * end "integrityCheckInfo" of type IntegrityCheckInfo begin "message" of type UL_DCCH_MessageType (CHOICE) [UNIVERSAL 31] begin "rrcConnectionReleaseComplete" of type RRCConnectionReleaseComplete (SEQUENCE) [UNIVERSAL 16] begin "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier (INTEGER) [UNIVERSAL 2] matching 0 against 0 end "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier end "rrcConnectionReleaseComplete" of type RRCConnectionReleaseComplete end "message" of type UL_DCCH_MessageType end "uL_DCCH_Message" of type UL_DCCH_Message end "uM_message" of type CHOICE end "car_RRC_ConnRelCmplUM" of type RLC_UM_DATA_IND Receive event:TSP1: [41] UM ? RLC_UM_DATA_IND = PDU (view PDU) Preliminary verdict:TSP1: [41] (PASS) Attach:[42] Enter Test Step ts_RRC_ConnRel::lt_RptRcvConnRel( 0 )
| StartTimer:[50] t_Dly [5000] 5000 ms 00:01:36.780 - Primitive: RLC_UM_DATA_IND: rrcConnectionReleaseComplete 00:01:36.780 - Primitive: RLC_UM_DATA_IND begin "car_RRC_ConnRelCmplUM" of type RLC_UM_DATA_IND (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "integrityResult" of type IntegrityResult (CHOICE) [UNIVERSAL 31] matching [integrityUsed: i_pass] against * end "integrityResult" of type IntegrityResult begin "uM_message" of type CHOICE [UNIVERSAL 31] begin "uL_DCCH_Message" of type UL_DCCH_Message (SEQUENCE) [UNIVERSAL 16] begin "integrityCheckInfo" of type IntegrityCheckInfo (SEQUENCE) [UNIVERSAL 16] matching { messageAuthenticationCode: '10111001101000110000011111000000'B , rrc_MessageSequenceNumber: 2 } against * end "integrityCheckInfo" of type IntegrityCheckInfo begin "message" of type UL_DCCH_MessageType (CHOICE) [UNIVERSAL 31] begin "rrcConnectionReleaseComplete" of type RRCConnectionReleaseComplete (SEQUENCE) [UNIVERSAL 16] begin "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier (INTEGER) [UNIVERSAL 2] matching 0 against 0 end "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier end "rrcConnectionReleaseComplete" of type RRCConnectionReleaseComplete end "message" of type UL_DCCH_MessageType end "uL_DCCH_Message" of type UL_DCCH_Message end "uM_message" of type CHOICE end "car_RRC_ConnRelCmplUM" of type RLC_UM_DATA_IND Assignment:TSP2: [53] tcv_K := 2 CancelTimer:TSP2: [53] t_Dly [5000] 5000 ms Receive event:TSP2: [53] UM ? RLC_UM_DATA_IND = PDU (view PDU) Preliminary verdict:TSP2: [53] (PASS) Attach:[42] Exit Test Step ts_RRC_ConnRel::lt_RptRcvConnRel
Attach:[3] Exit Test Step ts_RRC_ConnRel::lt_Send_RRC_ConnectionRelease
Attach:[4] Enter Test Step ts_RRC_ConnRel::lt_RestartCRLC_ForNextConnection( 0 )
| Attach:[7] Enter Test Step ts_CRLC_RelReconfSRB( 0 )
| Attach:[1] Enter Test Step ts_CRLC_Rel( -1 )
| 00:01:36.780 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:36.790 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 1 ]} Attach:[1] Exit Test Step ts_CRLC_Rel
Attach:[2] Enter Test Step ts_CRLC_Rel( -1 )
| 00:01:36.790 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:36.810 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 2 ]} Attach:[2] Exit Test Step ts_CRLC_Rel
Attach:[3] Enter Test Step ts_CRLC_Rel( -1 )
| 00:01:36.810 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:36.820 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 3 ]} Attach:[3] Exit Test Step ts_CRLC_Rel
Attach:[4] Enter Test Step ts_CRLC_Rel( -1 )
| 00:01:36.820 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:36.840 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 4 ]} Attach:[4] Exit Test Step ts_CRLC_Rel
Attach:[5] Enter Test Step ts_SS_RB1_ToRB4_Cfg( )
| 00:01:36.840 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:36.850 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 1 ]} 00:01:36.850 - Primitive: CRLC_Config_REQ Send event:[3] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:36.870 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[4] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 2 ]} 00:01:36.870 - Primitive: CRLC_Config_REQ Send event:[5] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:36.880 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[6] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 3 ]} 00:01:36.880 - Primitive: CRLC_Config_REQ Send event:[7] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:36.900 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[8] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 4 ]} Attach:[5] Exit Test Step ts_SS_RB1_ToRB4_Cfg
Attach:[7] Exit Test Step ts_CRLC_RelReconfSRB
Attach:[8] Enter Test Step ts_SetCellCfg( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Assignment:[2] cellConfig := cell_DCH_StandAloneSRB_NoConn Attach:[3] Enter Test Step ts_SaveCellInfo( 0 )
| Assignment:[2] tcv_CellInfoA := (view Assignment) Attach:[3] Exit Test Step ts_SaveCellInfo
Attach:[8] Exit Test Step ts_SetCellCfg
Attach:[4] Exit Test Step ts_RRC_ConnRel::lt_RestartCRLC_ForNextConnection
Attach:[5] Enter Test Step ts_SS_ResetSecurityKey( )
| Assignment:[1] tcv_CellIndInfo := (view Assignment) Assignment:[3] cipheringAlgorithmCapability := '0000000000000011'B Attach:[5] Exit Test Step ts_SS_ResetSecurityKey
Attach:[31] Exit Test Step ts_RRC_ConnRel
Attach:[15] Exit Test Step tc_12_4_1_2::lt_Attach_Steps_4To5
Attach:[16] Enter Test Step tc_12_4_1_2::lt_ActivateCellB_Step6( )
| Attach:[43] Enter Test Step ts_SS_DecrementCellPowerLevel( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[2] Enter Test Step ts_CheckCellIsConfigured( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[2] Exit Test Step ts_CheckCellIsConfigured
Assignment:[3] tcv_TmpAttenuationLvl := 10 Attach:[4] Enter Test Step ts_SS_DecrementCellPowerLevel::lt_CheckAttLevel( 0 )
| Preliminary verdict:[12] (PASS) Attach:[4] Exit Test Step ts_SS_DecrementCellPowerLevel::lt_CheckAttLevel
Attach:[5] Enter Test Step ts_SS_DecrementCellPowerLevel::lt_SetAttLevel( 0 )
| 00:01:36.900 - Primitive: CPHY_Cell_TxPower_Modify_REQ Send event:[8] CPHY ! CPHY_Cell_TxPower_Modify_REQ = PDU: { cellId: 0 , dLTxAttenuationLevel: 10 } 00:01:36.920 - Primitive: CPHY_Cell_TxPower_Modify_CNF begin "ca_CellTxPowerModiCnf" of type CPHY_Cell_TxPower_Modify_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER end "ca_CellTxPowerModiCnf" of type CPHY_Cell_TxPower_Modify_CNF Receive event:[9] CPHY ? CPHY_Cell_TxPower_Modify_CNF = PDU: { cellId: 0 } Attach:[5] Exit Test Step ts_SS_DecrementCellPowerLevel::lt_SetAttLevel
Assignment:[6] attenuationLevel := 10 Attach:[7] Enter Test Step ts_SaveCellInfo( 0 )
| Assignment:[2] tcv_CellInfoA := (view Assignment) Attach:[7] Exit Test Step ts_SaveCellInfo
Attach:[43] Exit Test Step ts_SS_DecrementCellPowerLevel
Attach:[44] Enter Test Step ts_SS_IncrementCellPowerLevel( 1 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 1 )
| Assignment:[4] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[2] Enter Test Step ts_CheckCellIsConfigured( 1 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 1 )
| Assignment:[4] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[2] Exit Test Step ts_CheckCellIsConfigured
Assignment:[3] tcv_TmpAttenuationLvl := 0 Attach:[4] Enter Test Step ts_SS_IncrementCellPowerLevel::lt_CheckAttLevel( 1 )
| Preliminary verdict:[12] (PASS) Attach:[4] Exit Test Step ts_SS_IncrementCellPowerLevel::lt_CheckAttLevel
Attach:[5] Enter Test Step ts_SS_IncrementCellPowerLevel::lt_SetAttLevel( 1 )
| 00:01:36.920 - Primitive: CPHY_Cell_TxPower_Modify_REQ Send event:[8] CPHY ! CPHY_Cell_TxPower_Modify_REQ = PDU: { cellId: 1 , dLTxAttenuationLevel: 0 } 00:01:36.930 - Primitive: CPHY_Cell_TxPower_Modify_CNF begin "ca_CellTxPowerModiCnf" of type CPHY_Cell_TxPower_Modify_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "cellId" of type INTEGER end "ca_CellTxPowerModiCnf" of type CPHY_Cell_TxPower_Modify_CNF Receive event:[9] CPHY ? CPHY_Cell_TxPower_Modify_CNF = PDU: { cellId: 1 } Attach:[5] Exit Test Step ts_SS_IncrementCellPowerLevel::lt_SetAttLevel
Assignment:[6] attenuationLevel := 0 Attach:[7] Enter Test Step ts_SaveCellInfo( 1 )
| Assignment:[4] tcv_CellInfoB := (view Assignment) Attach:[7] Exit Test Step ts_SaveCellInfo
Attach:[44] Exit Test Step ts_SS_IncrementCellPowerLevel
Attach:[16] Exit Test Step tc_12_4_1_2::lt_ActivateCellB_Step6
Attach:[17] Enter Test Step tc_12_4_1_2::lt_RARej_Steps_8To9( )
| Attach:[32] Enter Test Step ts_RRC_ConnEst( 1 )
| Attach:[1] Enter Test Step ts_SS_PrepareCellRRC_ConnEst( 1 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 1 )
| Assignment:[4] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[4] Enter Test Step ts_SS_PrepareCellRRC_ConnEst::lt_ReconfOldDPCH_Cell( 1 )
| Attach:[39] Enter Test Step ts_SS_RelDPCH( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[3] Enter Test Step ts_SS_RelDPCH::lt_RelSRB1_4( 0 )
| Attach:[119] Enter Test Step ts_CRLC_Rel( -1 )
| 00:01:36.930 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:36.950 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 1 ]} Attach:[119] Exit Test Step ts_CRLC_Rel
Attach:[120] Enter Test Step ts_CRLC_Rel( -1 )
| 00:01:36.950 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:36.960 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 2 ]} Attach:[120] Exit Test Step ts_CRLC_Rel
Attach:[121] Enter Test Step ts_CRLC_Rel( -1 )
| 00:01:36.960 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:36.980 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 3 ]} Attach:[121] Exit Test Step ts_CRLC_Rel
Attach:[122] Enter Test Step ts_CRLC_Rel( -1 )
| 00:01:36.980 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:36.990 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 4 ]} Attach:[122] Exit Test Step ts_CRLC_Rel
Attach:[3] Exit Test Step ts_SS_RelDPCH::lt_RelSRB1_4
Attach:[4] Enter Test Step ts_CMAC_Rel( -1 )
| 00:01:36.990 - Primitive: CMAC_Config_REQ Send event:[1] CMAC ! CMAC_Config_REQ = PDU (view PDU) 00:01:37.030 - Primitive: CMAC_Config_CNF begin "ca_CMAC_CfgCnf" of type CMAC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 26 against 26 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_CfgCnf" of type CMAC_Config_CNF Receive event:[2] CMAC ? CMAC_Config_CNF = PDU: { cellId: -1 , routingInfo: [physicalChannelIdentity: 26 ]} Attach:[4] Exit Test Step ts_CMAC_Rel
Attach:[5] Enter Test Step ts_CMAC_Rel( -1 )
| 00:01:37.030 - Primitive: CMAC_Config_REQ Send event:[1] CMAC ! CMAC_Config_REQ = PDU (view PDU) 00:01:37.060 - Primitive: CMAC_Config_CNF begin "ca_CMAC_CfgCnf" of type CMAC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 20 against 20 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_CfgCnf" of type CMAC_Config_CNF Receive event:[2] CMAC ? CMAC_Config_CNF = PDU: { cellId: -1 , routingInfo: [physicalChannelIdentity: 20 ]} Attach:[5] Exit Test Step ts_CMAC_Rel
Attach:[6] Enter Test Step ts_CPHY_TrChRelDCH_NoSHO( 0 )
| 00:01:37.060 - Primitive: CPHY_TrCH_Release_REQ Send event:[1] CPHY ! CPHY_TrCH_Release_REQ = PDU (view PDU) 00:01:37.070 - Primitive: CPHY_TrCH_Release_CNF begin "ca_PHY_RelCnf" of type CPHY_TrCH_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 26 against 26 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_PHY_RelCnf" of type CPHY_TrCH_Release_CNF Receive event:[2] CPHY ? CPHY_TrCH_Release_CNF = PDU (view PDU) Attach:[6] Exit Test Step ts_CPHY_TrChRelDCH_NoSHO
Attach:[7] Enter Test Step ts_CPHY_TrChRelDCH_NoSHO( 0 )
| 00:01:37.070 - Primitive: CPHY_TrCH_Release_REQ Send event:[1] CPHY ! CPHY_TrCH_Release_REQ = PDU (view PDU) 00:01:37.090 - Primitive: CPHY_TrCH_Release_CNF begin "ca_PHY_RelCnf" of type CPHY_TrCH_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 20 against 20 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_PHY_RelCnf" of type CPHY_TrCH_Release_CNF Receive event:[2] CPHY ? CPHY_TrCH_Release_CNF = PDU (view PDU) Attach:[7] Exit Test Step ts_CPHY_TrChRelDCH_NoSHO
Attach:[8] Enter Test Step ts_SS_StopRL( 0 )
| 00:01:37.090 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 26 ]} 00:01:37.100 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 26 against 26 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 26 ]} Attach:[8] Exit Test Step ts_SS_StopRL
Attach:[9] Enter Test Step ts_SS_StopRL( 0 )
| 00:01:37.100 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 20 ]} 00:01:37.130 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 20 against 20 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 20 ]} Attach:[9] Exit Test Step ts_SS_StopRL
Attach:[39] Exit Test Step ts_SS_RelDPCH
Assignment:[40] cellConfig := cell_NoDPCH Assignment:[40] DL_DPCH_SHO := GcFALSE Assignment:[40] UL_DPCH_SHO := GcFALSE Attach:[4] Exit Test Step ts_SS_PrepareCellRRC_ConnEst::lt_ReconfOldDPCH_Cell
Attach:[5] Enter Test Step ts_SS_AddDPCH( 1 )
| Attach:[1] Enter Test Step ts_SS_1DCH_DCCH_Cfg( 1 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 1 )
| Assignment:[4] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Assignment:[3] tcv_TGCFN := 0 00:01:37.130 - Primitive: CPHY_RL_Setup_REQ Send event:[4] CPHY ! CPHY_RL_Setup_REQ = PDU (view PDU) 00:01:37.150 - Primitive: CPHY_RL_Setup_CNF begin "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 26 against 26 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF Receive event:[5] CPHY ? CPHY_RL_Setup_CNF = PDU: { cellId: 1 , routingInfo: [physicalChannelIdentity: 26 ]} 00:01:37.150 - Primitive: CPHY_TrCH_Config_REQ Send event:[6] CPHY ! CPHY_TrCH_Config_REQ = PDU (view PDU) 00:01:37.180 - Primitive: CPHY_TrCH_Config_CNF begin "ca_TrChCfgCnf" of type CPHY_TrCH_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 26 against 26 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_TrChCfgCnf" of type CPHY_TrCH_Config_CNF Receive event:[7] CPHY ? CPHY_TrCH_Config_CNF = PDU (view PDU) 00:01:37.180 - Primitive: CMAC_Config_REQ Send event:[8] CMAC ! CMAC_Config_REQ = PDU (view PDU) 00:01:37.230 - Primitive: CMAC_Config_CNF begin "ca_CMAC_CfgCnf" of type CMAC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 26 against 26 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_CfgCnf" of type CMAC_Config_CNF Receive event:[9] CMAC ? CMAC_Config_CNF = PDU: { cellId: -1 , routingInfo: [physicalChannelIdentity: 26 ]} 00:01:37.230 - Primitive: CPHY_RL_Setup_REQ Send event:[10] CPHY ! CPHY_RL_Setup_REQ = PDU (view PDU) 00:01:37.240 - Primitive: CPHY_RL_Setup_CNF begin "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 20 against 20 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF Receive event:[11] CPHY ? CPHY_RL_Setup_CNF = PDU: { cellId: 1 , routingInfo: [physicalChannelIdentity: 20 ]} 00:01:37.240 - Primitive: CPHY_TrCH_Config_REQ Send event:[12] CPHY ! CPHY_TrCH_Config_REQ = PDU (view PDU) 00:01:37.290 - Primitive: CPHY_TrCH_Config_CNF begin "ca_TrChCfgCnf" of type CPHY_TrCH_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 20 against 20 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_TrChCfgCnf" of type CPHY_TrCH_Config_CNF Receive event:[13] CPHY ? CPHY_TrCH_Config_CNF = PDU (view PDU) 00:01:37.290 - Primitive: CMAC_Config_REQ Send event:[14] CMAC ! CMAC_Config_REQ = PDU (view PDU) 00:01:37.320 - Primitive: CMAC_Config_CNF begin "ca_CMAC_CfgCnf" of type CMAC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 20 against 20 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_CfgCnf" of type CMAC_Config_CNF Receive event:[15] CMAC ? CMAC_Config_CNF = PDU: { cellId: -1 , routingInfo: [physicalChannelIdentity: 20 ]} Attach:[1] Exit Test Step ts_SS_1DCH_DCCH_Cfg
Attach:[2] Enter Test Step ts_SS_RB1_ToRB4_Cfg( )
| 00:01:37.320 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:37.340 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 1 ]} 00:01:37.340 - Primitive: CRLC_Config_REQ Send event:[3] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:37.350 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[4] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 2 ]} 00:01:37.350 - Primitive: CRLC_Config_REQ Send event:[5] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:37.370 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[6] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 3 ]} 00:01:37.370 - Primitive: CRLC_Config_REQ Send event:[7] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:37.380 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[8] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 4 ]} Attach:[2] Exit Test Step ts_SS_RB1_ToRB4_Cfg
Attach:[5] Exit Test Step ts_SS_AddDPCH
Assignment:[6] cellConfig := cell_DCH_StandAloneSRB_NoConn Assignment:[6] DL_DPCH_SHO := GcTRUE Assignment:[6] UL_DPCH_SHO := GcTRUE Attach:[7] Enter Test Step ts_SaveCellInfo( 1 )
| Assignment:[4] tcv_CellInfoB := (view Assignment) Attach:[7] Exit Test Step ts_SaveCellInfo
Attach:[1] Exit Test Step ts_SS_PrepareCellRRC_ConnEst
Attach:[2] Enter Test Step ts_SetTmpCellInfo( 1 )
| Assignment:[4] tcv_TmpCellInfo := (view Assignment) Attach:[2] Exit Test Step ts_SetTmpCellInfo
Attach:[3] Enter Test Step ts_RRC_ConnEst::lt_RcvConnReq( 1 )
| 00:01:45.510 - Primitive: RLC_TR_DATA_IND: rrcConnectionRequest 00:01:45.510 - Primitive: RLC_TR_DATA_IND begin "car_RRC_ConnReq" of type RLC_TR_DATA_IND (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "tM_message" of type CHOICE [UNIVERSAL 31] begin "uL_CCCH_Message" of type UL_CCCH_Message (SEQUENCE) [UNIVERSAL 16] begin "message" of type UL_CCCH_MessageType (CHOICE) [UNIVERSAL 31] begin "rrcConnectionRequest" of type RRCConnectionRequest (SEQUENCE) [UNIVERSAL 16] begin "initialUE_Identity" of type InitialUE_Identity (CHOICE) [UNIVERSAL 31] begin InitialUE_Identity (CHOICE) [UNIVERSAL 31] end InitialUE_Identity begin InitialUE_Identity (CHOICE) [UNIVERSAL 31] begin "tmsi_and_LAI" of type TMSI_and_LAI_GSM_MAP (SEQUENCE) [UNIVERSAL 16] matching { tmsi: '00010001001000100011001101000100'B , lai: { plmn_Identity: { mcc: [ 0 , 0 , 1 ] , mnc: [ 0 , 1 ] } , lac: '0000000000000001'B } } against ? end "tmsi_and_LAI" of type TMSI_and_LAI_GSM_MAP end InitialUE_Identity matching [tmsi_and_LAI: { tmsi: '00010001001000100011001101000100'B , lai: { plmn_Identity: { mcc: [ 0 , 0 , 1 ] , mnc: [ 0 , 1 ] } , lac: '0000000000000001'B } } ] against ([imsi: ?], [tmsi_and_LAI: ?], [p_TMSI_and_RAI: ?], [imei: ?]) end "initialUE_Identity" of type InitialUE_Identity begin "establishmentCause" of type EstablishmentCause (ENUMERATED) [UNIVERSAL 10] matching registration against registration end "establishmentCause" of type EstablishmentCause begin "protocolErrorIndicator" of type ProtocolErrorIndicator (ENUMERATED) [UNIVERSAL 10] matching noError against noError end "protocolErrorIndicator" of type ProtocolErrorIndicator end "rrcConnectionRequest" of type RRCConnectionRequest end "message" of type UL_CCCH_MessageType end "uL_CCCH_Message" of type UL_CCCH_Message end "tM_message" of type CHOICE end "car_RRC_ConnReq" of type RLC_TR_DATA_IND Assignment:[7] tcv_InitialUE_Id := (view Assignment) Receive event:[7] TM ? RLC_TR_DATA_IND = PDU (view PDU) Attach:[3] Exit Test Step ts_RRC_ConnEst::lt_RcvConnReq
Attach:[4] Enter Test Step ts_RRC_ConnEst::lt_Send_ConnSetUp( 1 )
| 00:01:45.510 - Primitive: RLC_UM_DATA_REQ 00:01:45.530 - Primitive: RLC_UM_DATA_REQ: rrcConnectionSetup Send event:[31] UM ! RLC_UM_DATA_REQ = PDU (view PDU) Attach:[33] Enter Test Step ts_SetCellCfg( 1 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 1 )
| Assignment:[4] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Assignment:[2] cellConfig := cell_DCH_StandAloneSRB Attach:[3] Enter Test Step ts_SaveCellInfo( 1 )
| Assignment:[4] tcv_CellInfoB := (view Assignment) Attach:[3] Exit Test Step ts_SaveCellInfo
Attach:[33] Exit Test Step ts_SetCellCfg
Attach:[4] Exit Test Step ts_RRC_ConnEst::lt_Send_ConnSetUp
Attach:[5] Enter Test Step ts_RRC_ReceiveConnSetupCmpl( 1 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 1 )
| Assignment:[4] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
StartTimer:[3] t_WaitMS [13500] 13500 ms 00:01:46.040 - Primitive: RLC_AM_DATA_IND: rrcConnectionSetupComplete 00:01:46.060 - Primitive: RLC_AM_DATA_IND begin "car_RRC_ConnSetupCmpl" of type RLC_AM_DATA_IND (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "integrityResult" of type IntegrityResult (CHOICE) [UNIVERSAL 31] matching [integrityUsed: i_pass] against ? end "integrityResult" of type IntegrityResult begin "aM_message" of type CHOICE [UNIVERSAL 31] begin "uL_DCCH_Message" of type UL_DCCH_Message (SEQUENCE) [UNIVERSAL 16] begin "message" of type UL_DCCH_MessageType (CHOICE) [UNIVERSAL 31] begin "rrcConnectionSetupComplete" of type RRCConnectionSetupComplete (SEQUENCE) [UNIVERSAL 16] begin "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier (INTEGER) [UNIVERSAL 2] matching 0 against 0 end "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier begin "startList" of type STARTList (SEQUENCEOF) [UNIVERSAL 28] matching [ { cn_DomainIdentity: ps_domain, start_Value: '00000000000000000010'B } , { cn_DomainIdentity: cs_domain, start_Value: '00000000000000000010'B } ] against ? end "startList" of type STARTList begin "ue_RadioAccessCapability" of type UE_RadioAccessCapability (SEQUENCE) [UNIVERSAL 16] matching { accessStratumReleaseIndicator: r99, pdcp_Capability: { losslessSRNS_RelocationSupport: GcFALSE , supportForRfc2507: [notSupported: NULL]} , rlc_Capability: { totalRLC_AM_BufferSize: kb50, maximumRLC_WindowSize: mws2047, maximumAM_EntityNumber: am6} , transportChannelCapability: { dl_TransChCapability: { maxNoBitsReceived: b8960, maxConvCodeBitsReceived: b1280, turboDecodingSupport: [supported: b8960], maxSimultaneousTransChs: e8, maxSimultaneousCCTrCH_Count: 1 , maxReceivedTransportBlocks: tb32, maxNumberOfTFC: tfc128, maxNumberOfTF: tf64} , ul_TransChCapability: { maxNoBitsTransmitted: b3840, maxConvCodeBitsTransmitted: b1280, turboEncodingSupport: [supported: b3840], maxSimultaneousTransChs: e8, modeSpecificInfo: [fdd: NULL], maxTransmittedBlocks: tb32, maxNumberOfTFC: tfc64, maxNumberOfTF: tf32} } , rf_Capability: { fddRF_Capability: { ue_PowerClass: 4 , txRxFrequencySeparation: mhz190} , tddRF_Capability: OMIT} , physicalChannelCapability: { fddPhysChCapability: { downlinkPhysChCapability: { maxNoDPCH_PDSCH_Codes: 1 , maxNoPhysChBitsReceived: b9600, supportForSF_512: GcFALSE , supportOfPDSCH: GcFALSE , simultaneousSCCPCH_DPCH_Reception: [notSupported: NULL]} , uplinkPhysChCapability: { maxNoDPDCH_BitsTransmitted: b4800, supportOfPCPCH: GcFALSE } } , tddPhysChCapability: OMIT} , ue_MultiModeRAT_Capability: { multiRAT_CapabilityList: { supportOfGSM: GcFALSE , supportOfMulticarrier: GcFALSE } , multiModeCapability: fdd} , securityCapability: { cipheringAlgorithmCap: '0000000000000011'B , integrityProtectionAlgorithmCap: '0000000000000010'B } , ue_positioning_Capability: { standaloneLocMethodsSupported: GcFALSE , ue_BasedOTDOA_Supported: GcFALSE , networkAssistedGPS_Supported: noNetworkAssistedGPS, supportForUE_GPS_TimingOfCellFrames: GcFALSE , supportForIPDL: GcFALSE } , measurementCapability: { downlinkCompressedMode: { fdd_Measurements: GcTRUE , tdd_Measurements: OMIT, gsm_Measurements: { gsm900: GcTRUE , dcs1800: GcTRUE , gsm1900: GcTRUE } , multiCarrierMeasurements: GcFALSE } , uplinkCompressedMode: { fdd_Measurements: GcTRUE , tdd_Measurements: OMIT, gsm_Measurements: { gsm900: GcTRUE , dcs1800: GcTRUE , gsm1900: GcTRUE } , multiCarrierMeasurements: GcFALSE } } } against * end "ue_RadioAccessCapability" of type UE_RadioAccessCapability end "rrcConnectionSetupComplete" of type RRCConnectionSetupComplete end "message" of type UL_DCCH_MessageType end "uL_DCCH_Message" of type UL_DCCH_Message end "aM_message" of type CHOICE end "car_RRC_ConnSetupCmpl" of type RLC_AM_DATA_IND Assignment:TSP1: [5] tcv_StartList := (view Assignment) Assignment:TSP1: [5] cipheringAlgorithmCapability := '0000000000000011'B CancelTimer:TSP1: [5] t_WaitMS [13500] 13500 ms Receive event:TSP1: [5] AM ? RLC_AM_DATA_IND = PDU (view PDU) Preliminary verdict:TSP1: [5] (PASS) Attach:[6] Enter Test Step ts_RRC_ReceiveConnSetupCmpl::lt_GetHFN( 1 )
| Assignment:[13] tcv_Count := 2 Attach:[17] Enter Test Step ts_RRC_ReceiveConnSetupCmpl::lt_FirstValue( 1 )
| Assignment:[23] start_PS := '00000000000000000010'B Attach:[17] Exit Test Step ts_RRC_ReceiveConnSetupCmpl::lt_FirstValue
Attach:[18] Enter Test Step ts_RRC_ReceiveConnSetupCmpl::lt_SecondValue( 1 )
| Assignment:[26] start_CS := '00000000000000000010'B Attach:[18] Exit Test Step ts_RRC_ReceiveConnSetupCmpl::lt_SecondValue
Attach:[6] Exit Test Step ts_RRC_ReceiveConnSetupCmpl::lt_GetHFN
Attach:[5] Exit Test Step ts_RRC_ReceiveConnSetupCmpl
Attach:[32] Exit Test Step ts_RRC_ConnEst
00:01:46.040 - Primitive: RLC_AM_DATA_IND: initialDirectTransfer 00:01:46.040 - Primitive: RRC_DATA_IND: gmm:routingAreaUpdateRequest begin "car_PS_InitDirectTransfer" of type RRC_DataInd (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "rB_Id" of type SS_RB_Identity (INTEGER) [UNIVERSAL 2] matching 3 against 3 end "rB_Id" of type SS_RB_Identity begin "cN_Domain" of type SS_CN_DomainIdentity (INTEGER) [UNIVERSAL 2] matching 1 against 1 end "cN_Domain" of type SS_CN_DomainIdentity begin "start" of type START_Value (BITSTRING) [UNIVERSAL 3] matching '00000000000000000010'B against ? end "start" of type START_Value begin "msg" of type ROUTINGAREAUPDATEREQUEST (SEQUENCE) [UNIVERSAL 16] begin "skipIndicator" of type SkipIndicator (BITSTRING) [UNIVERSAL 3] matching '0000'B against '0000'B end "skipIndicator" of type SkipIndicator begin "gMMProtocolDiscriminator" of type ProtocolDiscriminator (BITSTRING) [UNIVERSAL 3] matching '1000'B against '1000'B end "gMMProtocolDiscriminator" of type ProtocolDiscriminator begin "msgType" of type MsgType (BITSTRING) [UNIVERSAL 3] matching '00001000'B against '00001000'B end "msgType" of type MsgType begin "gprsCiphKeySeqNo" of type CiphKeySeqNum (SEQUENCE) [UNIVERSAL 16] begin "spare1" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against '0'B end "spare1" of type B1 begin "keySeq" of type KeySeq (BITSTRING) [UNIVERSAL 3] matching '001'B against '001'B end "keySeq" of type KeySeq end "gprsCiphKeySeqNo" of type CiphKeySeqNum begin "updateType" of type UpdateType_v (SEQUENCE) [UNIVERSAL 16] begin "for" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against '0'B end "for" of type B1 begin "value" of type B3 (BITSTRING) [UNIVERSAL 3] matching '000'B against '000'B end "value" of type B3 end "updateType" of type UpdateType_v begin "oldRAI" of type RAI_v (SEQUENCE) [UNIVERSAL 16] begin "plmn" of type OCTETSTRING [UNIVERSAL 4] matching '00F110'O against '00F110'O end "plmn" of type OCTETSTRING begin "lac" of type OCTETSTRING [UNIVERSAL 4] matching '0001'O against '0001'O end "lac" of type OCTETSTRING begin "rac" of type OCTETSTRING [UNIVERSAL 4] matching '05'O against '05'O end "rac" of type OCTETSTRING end "oldRAI" of type RAI_v begin "msRadioAccessCap" of type MSRadioAccessCap_lv (SEQUENCE) [UNIVERSAL 16] matching { iel: '0B'O , value: '15F38233542A332644A198'O } against * end "msRadioAccessCap" of type MSRadioAccessCap_lv begin "readyTimer" of type GPRS_Timer (SEQUENCE) [UNIVERSAL 16] begin "iei" of type IEI8 (BITSTRING) [UNIVERSAL 3] matching '00010111'B against '00010111'B end "iei" of type IEI8 begin "unit" of type B3 (BITSTRING) [UNIVERSAL 3] matching '000'B against ? end "unit" of type B3 begin "value" of type B5 (BITSTRING) [UNIVERSAL 3] matching '10110'B against ? end "value" of type B5 end "readyTimer" of type GPRS_Timer begin "drxParameter" of type DRXparamter_tv (SEQUENCE) [UNIVERSAL 16] begin "iei" of type IEI8 (BITSTRING) [UNIVERSAL 3] matching '00100111'B against '00100111'B end "iei" of type IEI8 begin "splitPGcycleCode" of type B8 (BITSTRING) [UNIVERSAL 3] matching '00000111'B against ? end "splitPGcycleCode" of type B8 begin "cnDRXcoef" of type B4 (BITSTRING) [UNIVERSAL 3] matching '0000'B against ? end "cnDRXcoef" of type B4 begin "splitOnCCCH" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against ? end "splitOnCCCH" of type B1 begin "nonDRXtimer" of type B3 (BITSTRING) [UNIVERSAL 3] matching '100'B against ? end "nonDRXtimer" of type B3 end "drxParameter" of type DRXparamter_tv begin "ptmsi" of type GMM_MS_IdentityPTMSI (SEQUENCE) [UNIVERSAL 16] begin "iei" of type IEI8 (BITSTRING) [UNIVERSAL 3] matching '00011000'B against '00011000'B end "iei" of type IEI8 begin "iel" of type Length (OCTETSTRING) [UNIVERSAL 4] matching '05'O against '05'O end "iel" of type Length begin "iDigit1" of type B4 (BITSTRING) [UNIVERSAL 3] matching '1111'B against '1111'B end "iDigit1" of type B4 begin "oddEvenInd" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against '0'B end "oddEvenInd" of type B1 begin "typeOfId" of type B3 (BITSTRING) [UNIVERSAL 3] matching '100'B against '100'B end "typeOfId" of type B3 begin "otherDigits" of type OCTETSTRING [UNIVERSAL 4] matching '12345678'O against ? end "otherDigits" of type OCTETSTRING end "ptmsi" of type GMM_MS_IdentityPTMSI begin "msnetworkcap" of type MS_NetworkCap_tlv (SEQUENCE) [UNIVERSAL 16] matching { iei: '00110001'B , iel: '02'O , value: 'E540'O } against * end "msnetworkcap" of type MS_NetworkCap_tlv begin "pDP_ContextStatus" of type PDP_ContextStatus (SEQUENCE) [UNIVERSAL 16] matching { iei: '00110010'B , iel: '02'O , nSAPI: '0000000000000000'B } against * end "pDP_ContextStatus" of type PDP_ContextStatus end "msg" of type ROUTINGAREAUPDATEREQUEST end "car_PS_InitDirectTransfer" of type RRC_DataInd Assignment:[33] tcv_Start := '00000000000000000010'B Receive event:[33] Dc ? RRC_DataInd = PDU (view PDU) Attach:[34] Enter Test Step ts_SS_SecurityDownloadStart( ps_domain )
| Assignment:[4] start_PS := '00000000000000000010'B Attach:[34] Exit Test Step ts_SS_SecurityDownloadStart
00:01:46.120 - Primitive: RRC_DATA_REQ: gmm:routingAreaUpdateReject 00:01:46.120 - Primitive: RLC_AM_DATA_REQ:downlinkDirectTransfer Send event:[35] Dc ! RRC_DataReq = PDU (view PDU) Attach:[36] Enter Test Step ts_RRC_ConnRel( 1 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 1 )
| Assignment:[4] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[2] Enter Test Step ts_RRC_Delay( 1000 )
| StartTimer:[1] t_Dly [5000] 1000 ms Timed out Timer:t_Dly TimeOut:[2] t_Dly [5000] 1000 ms Attach:[2] Exit Test Step ts_RRC_Delay
Attach:[3] Enter Test Step ts_RRC_ConnRel::lt_Send_RRC_ConnectionRelease( 1 )
| Assignment:[39] tcv_N308 := 1 Assignment:[39] tcv_K := 1 00:01:47.120 - Primitive: RLC_UM_DATA_REQ 00:01:47.120 - Primitive: RLC_UM_DATA_REQ: rrcConnectionRelease Send event:[40] UM ! RLC_UM_DATA_REQ = PDU (view PDU) 00:01:47.380 - Primitive: RLC_UM_DATA_IND: rrcConnectionReleaseComplete 00:01:47.380 - Primitive: RLC_UM_DATA_IND begin "car_RRC_ConnRelCmplUM" of type RLC_UM_DATA_IND (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "integrityResult" of type IntegrityResult (CHOICE) [UNIVERSAL 31] matching [integrityUsed: i_pass] against * end "integrityResult" of type IntegrityResult begin "uM_message" of type CHOICE [UNIVERSAL 31] begin "uL_DCCH_Message" of type UL_DCCH_Message (SEQUENCE) [UNIVERSAL 16] begin "message" of type UL_DCCH_MessageType (CHOICE) [UNIVERSAL 31] begin "rrcConnectionReleaseComplete" of type RRCConnectionReleaseComplete (SEQUENCE) [UNIVERSAL 16] begin "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier (INTEGER) [UNIVERSAL 2] matching 0 against 0 end "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier end "rrcConnectionReleaseComplete" of type RRCConnectionReleaseComplete end "message" of type UL_DCCH_MessageType end "uL_DCCH_Message" of type UL_DCCH_Message end "uM_message" of type CHOICE end "car_RRC_ConnRelCmplUM" of type RLC_UM_DATA_IND Receive event:TSP1: [41] UM ? RLC_UM_DATA_IND = PDU (view PDU) Preliminary verdict:TSP1: [41] (PASS) Attach:[42] Enter Test Step ts_RRC_ConnRel::lt_RptRcvConnRel( 1 )
| StartTimer:[50] t_Dly [5000] 5000 ms 00:01:47.560 - Primitive: RLC_UM_DATA_IND: rrcConnectionReleaseComplete 00:01:47.560 - Primitive: RLC_UM_DATA_IND begin "car_RRC_ConnRelCmplUM" of type RLC_UM_DATA_IND (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "integrityResult" of type IntegrityResult (CHOICE) [UNIVERSAL 31] matching [integrityUsed: i_pass] against * end "integrityResult" of type IntegrityResult begin "uM_message" of type CHOICE [UNIVERSAL 31] begin "uL_DCCH_Message" of type UL_DCCH_Message (SEQUENCE) [UNIVERSAL 16] begin "message" of type UL_DCCH_MessageType (CHOICE) [UNIVERSAL 31] begin "rrcConnectionReleaseComplete" of type RRCConnectionReleaseComplete (SEQUENCE) [UNIVERSAL 16] begin "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier (INTEGER) [UNIVERSAL 2] matching 0 against 0 end "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier end "rrcConnectionReleaseComplete" of type RRCConnectionReleaseComplete end "message" of type UL_DCCH_MessageType end "uL_DCCH_Message" of type UL_DCCH_Message end "uM_message" of type CHOICE end "car_RRC_ConnRelCmplUM" of type RLC_UM_DATA_IND Assignment:TSP2: [53] tcv_K := 2 CancelTimer:TSP2: [53] t_Dly [5000] 5000 ms Receive event:TSP2: [53] UM ? RLC_UM_DATA_IND = PDU (view PDU) Preliminary verdict:TSP2: [53] (PASS) Attach:[42] Exit Test Step ts_RRC_ConnRel::lt_RptRcvConnRel
Attach:[3] Exit Test Step ts_RRC_ConnRel::lt_Send_RRC_ConnectionRelease
Attach:[4] Enter Test Step ts_RRC_ConnRel::lt_RestartCRLC_ForNextConnection( 1 )
| Attach:[7] Enter Test Step ts_CRLC_RelReconfSRB( 1 )
| Attach:[1] Enter Test Step ts_CRLC_Rel( -1 )
| 00:01:47.560 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:47.570 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 1 ]} Attach:[1] Exit Test Step ts_CRLC_Rel
Attach:[2] Enter Test Step ts_CRLC_Rel( -1 )
| 00:01:47.570 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:47.590 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 2 ]} Attach:[2] Exit Test Step ts_CRLC_Rel
Attach:[3] Enter Test Step ts_CRLC_Rel( -1 )
| 00:01:47.590 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:47.600 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 3 ]} Attach:[3] Exit Test Step ts_CRLC_Rel
Attach:[4] Enter Test Step ts_CRLC_Rel( -1 )
| 00:01:47.600 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:47.620 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 4 ]} Attach:[4] Exit Test Step ts_CRLC_Rel
Attach:[5] Enter Test Step ts_SS_RB1_ToRB4_Cfg( )
| 00:01:47.620 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:47.630 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 1 ]} 00:01:47.630 - Primitive: CRLC_Config_REQ Send event:[3] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:47.650 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[4] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 2 ]} 00:01:47.650 - Primitive: CRLC_Config_REQ Send event:[5] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:47.670 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[6] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 3 ]} 00:01:47.670 - Primitive: CRLC_Config_REQ Send event:[7] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:47.680 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[8] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 4 ]} Attach:[5] Exit Test Step ts_SS_RB1_ToRB4_Cfg
Attach:[7] Exit Test Step ts_CRLC_RelReconfSRB
Attach:[8] Enter Test Step ts_SetCellCfg( 1 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 1 )
| Assignment:[4] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Assignment:[2] cellConfig := cell_DCH_StandAloneSRB_NoConn Attach:[3] Enter Test Step ts_SaveCellInfo( 1 )
| Assignment:[4] tcv_CellInfoB := (view Assignment) Attach:[3] Exit Test Step ts_SaveCellInfo
Attach:[8] Exit Test Step ts_SetCellCfg
Attach:[4] Exit Test Step ts_RRC_ConnRel::lt_RestartCRLC_ForNextConnection
Attach:[5] Enter Test Step ts_SS_ResetSecurityKey( )
| Assignment:[1] tcv_CellIndInfo := (view Assignment) Assignment:[3] cipheringAlgorithmCapability := '0000000000000011'B Attach:[5] Exit Test Step ts_SS_ResetSecurityKey
Attach:[36] Exit Test Step ts_RRC_ConnRel
Attach:[17] Exit Test Step tc_12_4_1_2::lt_RARej_Steps_8To9
Attach:[18] Enter Test Step ts_GMM_InitVariablesPS( )
| Assignment:[1] tcv_CN_Domain := ps_domain Assignment:[1] tcv_RAB_Id := '00000101'B Assignment:[2] tcv_RRC_RAB_Type := cell_DCH_64kPS_RAB_SRB Attach:[3] Enter Test Step ts_GMM_InitVariablesPS::lt_RRC_InitServVarPS( )
| Assignment:[5] tcv_RRC_PagingCau := terminatingInteractiveCall Assignment:[5] tcv_RRC_EstCauMO := originatingInteractiveCall Assignment:[5] tcv_RRC_EstCauMT := terminatingInteractiveCall Attach:[3] Exit Test Step ts_GMM_InitVariablesPS::lt_RRC_InitServVarPS
Attach:[18] Exit Test Step ts_GMM_InitVariablesPS
Attach:[19] Enter Test Step ts_PS_Paging_PTMSI( 1 )
| Attach:[1] Enter Test Step ts_NAS_Delay( 5000 )
| StartTimer:[1] t_Dly [5000] 5000 ms Timed out Timer:t_Dly TimeOut:[2] t_Dly [5000] 5000 ms Attach:[1] Exit Test Step ts_NAS_Delay
Attach:[2] Enter Test Step ts_CMAC_Pag1_Cfg( 1 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 1 )
| Assignment:[4] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[3] Enter Test Step ts_CMAC_Pag1_Cfg::lt_CalculateDrxCycleLength( 1 )
| Assignment:[10] tcv_dRX_CycleLengthPaging := 7 Attach:[3] Exit Test Step ts_CMAC_Pag1_Cfg::lt_CalculateDrxCycleLength
00:01:52.700 - Primitive: CMAC_PAGING_Config_REQ Send event:[4] CMAC ! CMAC_PAGING_Config_REQ = PDU (view PDU) 00:01:52.710 - Primitive: CMAC_PAGING_Config_CNF begin "ca_CMAC_PagingCfgCnf" of type CMAC_PAGING_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 5 against 5 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_PagingCfgCnf" of type CMAC_PAGING_Config_CNF Receive event:[5] CMAC ? CMAC_PAGING_Config_CNF = PDU (view PDU) Attach:[2] Exit Test Step ts_CMAC_Pag1_Cfg
00:01:52.710 - Primitive: RLC_TR_DATA_REQ 00:01:52.710 - Primitive: RLC_TR_DATA_REQ: pagingType1 Send event:[3] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[19] Exit Test Step ts_PS_Paging_PTMSI
Attach:[20] Enter Test Step ts_VerifyNoAccess( 10 )
| StartTimer:[3] t_WaitS [15] 10 s Timed out Timer:t_WaitS TimeOut:[5] t_WaitS [15] 10 s Preliminary verdict:[5] (PASS) Attach:[20] Exit Test Step ts_VerifyNoAccess
Attach:[21] Enter Test Step tc_12_4_1_2::lt_ActivateCellD_Step12( )
| Attach:[45] Enter Test Step ts_SS_StopCell( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[4] Enter Test Step ts_SS_StopRL( 0 )
| 00:02:02.710 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 4 ]} 00:02:02.730 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 4 ]} Attach:[4] Exit Test Step ts_SS_StopRL
Attach:[5] Enter Test Step ts_SS_StopCellExcept_pCCPCH( 0 )
| Attach:[1] Enter Test Step ts_SS_StopRL( 0 )
| 00:02:02.730 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 1 ]} 00:02:02.740 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 1 ]} Attach:[1] Exit Test Step ts_SS_StopRL
Attach:[2] Enter Test Step ts_SS_StopRL( 0 )
| 00:02:02.740 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 2 ]} 00:02:02.760 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 2 ]} Attach:[2] Exit Test Step ts_SS_StopRL
Attach:[3] Enter Test Step ts_SS_StopRL( 0 )
| 00:02:02.760 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 0 ]} 00:02:02.780 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 0 ]} Attach:[3] Exit Test Step ts_SS_StopRL
Attach:[4] Enter Test Step ts_SS_StopRL( 0 )
| 00:02:02.780 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 8 ]} 00:02:02.790 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 8 against 8 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 8 ]} Attach:[4] Exit Test Step ts_SS_StopRL
Attach:[5] Enter Test Step ts_SS_StopRL( 0 )
| 00:02:02.790 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 7 ]} 00:02:02.810 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 7 against 7 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 7 ]} Attach:[5] Exit Test Step ts_SS_StopRL
Attach:[6] Enter Test Step ts_SS_StopRL( 0 )
| 00:02:02.810 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 6 ]} 00:02:02.820 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 6 ]} Attach:[6] Exit Test Step ts_SS_StopRL
Attach:[7] Enter Test Step ts_SS_StopRL( 0 )
| 00:02:02.820 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 5 ]} 00:02:02.840 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 5 against 5 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 5 ]} Attach:[7] Exit Test Step ts_SS_StopRL
Attach:[9] Enter Test Step ts_SS_StopRL( 0 )
| 00:02:02.840 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 26 ]} 00:02:02.850 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 26 against 26 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 26 ]} Attach:[9] Exit Test Step ts_SS_StopRL
Attach:[10] Enter Test Step ts_SS_StopRL( 0 )
| 00:02:02.850 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 20 ]} 00:02:02.870 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 20 against 20 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 20 ]} Attach:[10] Exit Test Step ts_SS_StopRL
Attach:[5] Exit Test Step ts_SS_StopCellExcept_pCCPCH
Attach:[6] Enter Test Step ts_SetCellCfg( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Assignment:[2] cellConfig := cell_NotConfigured Attach:[3] Enter Test Step ts_SaveCellInfo( 0 )
| Assignment:[2] tcv_CellInfoA := (view Assignment) Attach:[3] Exit Test Step ts_SaveCellInfo
Attach:[6] Exit Test Step ts_SetCellCfg
Attach:[45] Exit Test Step ts_SS_StopCell
Attach:[46] Enter Test Step ts_SS_DecrementCellPowerLevel( 1 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 1 )
| Assignment:[4] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[2] Enter Test Step ts_CheckCellIsConfigured( 1 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 1 )
| Assignment:[4] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[2] Exit Test Step ts_CheckCellIsConfigured
Assignment:[3] tcv_TmpAttenuationLvl := 30 Attach:[4] Enter Test Step ts_SS_DecrementCellPowerLevel::lt_CheckAttLevel( 1 )
| Preliminary verdict:[12] (PASS) Attach:[4] Exit Test Step ts_SS_DecrementCellPowerLevel::lt_CheckAttLevel
Attach:[5] Enter Test Step ts_SS_DecrementCellPowerLevel::lt_SetAttLevel( 1 )
| 00:02:02.870 - Primitive: CPHY_Cell_TxPower_Modify_REQ Send event:[8] CPHY ! CPHY_Cell_TxPower_Modify_REQ = PDU: { cellId: 1 , dLTxAttenuationLevel: 30 } 00:02:02.880 - Primitive: CPHY_Cell_TxPower_Modify_CNF begin "ca_CellTxPowerModiCnf" of type CPHY_Cell_TxPower_Modify_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "cellId" of type INTEGER end "ca_CellTxPowerModiCnf" of type CPHY_Cell_TxPower_Modify_CNF Receive event:[9] CPHY ? CPHY_Cell_TxPower_Modify_CNF = PDU: { cellId: 1 } Attach:[5] Exit Test Step ts_SS_DecrementCellPowerLevel::lt_SetAttLevel
Assignment:[6] attenuationLevel := 30 Attach:[7] Enter Test Step ts_SaveCellInfo( 1 )
| Assignment:[4] tcv_CellInfoB := (view Assignment) Attach:[7] Exit Test Step ts_SaveCellInfo
Attach:[46] Exit Test Step ts_SS_DecrementCellPowerLevel
Attach:[47] Enter Test Step ts_SS_CreateCellDCH( 3 )
| Attach:[1] Enter Test Step ts_SS_CellCfg( 3 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 3 )
| Assignment:[8] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[4] Enter Test Step ts_SS_CellCfg::lt_CelllsAlreadyStarted( 3 )
| Attach:[11] Enter Test Step ts_CountConfiguredCell( )
| Assignment:[1] tcv_NumCfgCell := 0 Attach:[2] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 0 , frequenc ...
| (view Test Step parameters) Attach:[2] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[3] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 1 , frequenc ...
| (view Test Step parameters) Assignment:[11] tcv_NumCfgCell := 1 Attach:[3] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[4] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 2 , frequenc ...
| (view Test Step parameters) Attach:[4] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[5] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 3 , frequenc ...
| (view Test Step parameters) Attach:[5] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[6] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 4 , frequenc ...
| (view Test Step parameters) Attach:[6] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[7] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 5 , frequenc ...
| (view Test Step parameters) Attach:[7] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[8] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 6 , frequenc ...
| (view Test Step parameters) Attach:[8] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[9] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 7 , frequenc ...
| (view Test Step parameters) Attach:[9] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[11] Exit Test Step ts_CountConfiguredCell
Attach:[4] Exit Test Step ts_SS_CellCfg::lt_CelllsAlreadyStarted
00:02:02.880 - Primitive: CPHY_Cell_Config_REQ Send event:[6] CPHY ! CPHY_Cell_Config_REQ = PDU (view PDU) 00:02:02.900 - Primitive: CPHY_Cell_Config_CNF begin "ca_CellCfgCnf" of type CPHY_Cell_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER end "ca_CellCfgCnf" of type CPHY_Cell_Config_CNF Receive event:[7] CPHY ? CPHY_Cell_Config_CNF = PDU: { cellId: 3 } Attach:[8] Enter Test Step ts_SaveCellInfo( 3 )
| Assignment:[8] tcv_CellInfoD := (view Assignment) Attach:[8] Exit Test Step ts_SaveCellInfo
Attach:[1] Exit Test Step ts_SS_CellCfg
Attach:[2] Enter Test Step ts_SS_BCH_SCH_CPICH_Cfg( 3 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 3 )
| Assignment:[8] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
00:02:02.900 - Primitive: CPHY_RL_Setup_REQ Send event:[3] CPHY ! CPHY_RL_Setup_REQ = PDU (view PDU) 00:02:02.920 - Primitive: CPHY_RL_Setup_CNF begin "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF Receive event:[4] CPHY ? CPHY_RL_Setup_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 0 ]} 00:02:03.170 - Primitive: CPHY_RL_Setup_REQ Send event:[5] CPHY ! CPHY_RL_Setup_REQ = PDU (view PDU) 00:02:03.200 - Primitive: CPHY_RL_Setup_CNF begin "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF Receive event:[6] CPHY ? CPHY_RL_Setup_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 1 ]} 00:02:03.200 - Primitive: CPHY_RL_Setup_REQ Send event:[7] CPHY ! CPHY_RL_Setup_REQ = PDU (view PDU) 00:02:03.210 - Primitive: CPHY_RL_Setup_CNF begin "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF Receive event:[8] CPHY ? CPHY_RL_Setup_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 2 ]} 00:02:03.210 - Primitive: CPHY_RL_Setup_REQ Send event:[9] CPHY ! CPHY_RL_Setup_REQ = PDU (view PDU) 00:02:03.240 - Primitive: CPHY_RL_Setup_CNF begin "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF Receive event:[10] CPHY ? CPHY_RL_Setup_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 4 ]} 00:02:03.240 - Primitive: CPHY_TrCH_Config_REQ Send event:[11] CPHY ! CPHY_TrCH_Config_REQ = PDU (view PDU) 00:02:03.290 - Primitive: CPHY_TrCH_Config_CNF begin "ca_TrChCfgCnf" of type CPHY_TrCH_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_TrChCfgCnf" of type CPHY_TrCH_Config_CNF Receive event:[12] CPHY ? CPHY_TrCH_Config_CNF = PDU (view PDU) 00:02:03.290 - Primitive: CMAC_Config_REQ Send event:[13] CMAC ! CMAC_Config_REQ = PDU (view PDU) 00:02:03.320 - Primitive: CMAC_Config_CNF begin "ca_CMAC_CfgCnf" of type CMAC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_CfgCnf" of type CMAC_Config_CNF Receive event:[14] CMAC ? CMAC_Config_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 4 ]} Attach:[2] Exit Test Step ts_SS_BCH_SCH_CPICH_Cfg
Attach:[3] Enter Test Step ts_SS_PCH_FACH_CCCH_Cfg( 3 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 3 )
| Assignment:[8] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
00:02:03.320 - Primitive: CPHY_RL_Setup_REQ Send event:[3] CPHY ! CPHY_RL_Setup_REQ = PDU (view PDU) 00:02:03.350 - Primitive: CPHY_RL_Setup_CNF begin "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 5 against 5 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF Receive event:[4] CPHY ? CPHY_RL_Setup_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 5 ]} 00:02:03.350 - Primitive: CPHY_TrCH_Config_REQ Send event:[5] CPHY ! CPHY_TrCH_Config_REQ = PDU (view PDU) 00:02:03.380 - Primitive: CPHY_TrCH_Config_CNF begin "ca_TrChCfgCnf" of type CPHY_TrCH_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 5 against 5 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_TrChCfgCnf" of type CPHY_TrCH_Config_CNF Receive event:[6] CPHY ? CPHY_TrCH_Config_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 5 ]} 00:02:03.380 - Primitive: CMAC_Config_REQ Send event:[7] CMAC ! CMAC_Config_REQ = PDU (view PDU) 00:02:03.400 - Primitive: CMAC_Config_CNF begin "ca_CMAC_CfgCnf" of type CMAC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 5 against 5 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_CfgCnf" of type CMAC_Config_CNF Receive event:[8] CMAC ? CMAC_Config_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 5 ]} 00:02:03.400 - Primitive: CPHY_RL_Setup_REQ Send event:[9] CPHY ! CPHY_RL_Setup_REQ = PDU (view PDU) 00:02:03.420 - Primitive: CPHY_RL_Setup_CNF begin "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF Receive event:[10] CPHY ? CPHY_RL_Setup_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 6 ]} Attach:[3] Exit Test Step ts_SS_PCH_FACH_CCCH_Cfg
Attach:[4] Enter Test Step ts_SS_RACH_CCCH_Cfg( 3 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 3 )
| Assignment:[8] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
00:02:03.420 - Primitive: CPHY_RL_Setup_REQ Send event:[3] CPHY ! CPHY_RL_Setup_REQ = PDU (view PDU) 00:02:03.430 - Primitive: CPHY_RL_Setup_CNF begin "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 7 against 7 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF Receive event:[4] CPHY ? CPHY_RL_Setup_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 7 ]} 00:02:03.430 - Primitive: CPHY_RL_Setup_REQ Send event:[5] CPHY ! CPHY_RL_Setup_REQ = PDU (view PDU) 00:02:03.450 - Primitive: CPHY_RL_Setup_CNF begin "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 8 against 8 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF Receive event:[6] CPHY ? CPHY_RL_Setup_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 8 ]} 00:02:03.450 - Primitive: CPHY_TrCH_Config_REQ Send event:[7] CPHY ! CPHY_TrCH_Config_REQ = PDU (view PDU) 00:02:03.490 - Primitive: CPHY_TrCH_Config_CNF begin "ca_TrChCfgCnf" of type CPHY_TrCH_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 8 against 8 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_TrChCfgCnf" of type CPHY_TrCH_Config_CNF Receive event:[8] CPHY ? CPHY_TrCH_Config_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 8 ]} 00:02:03.490 - Primitive: CMAC_Config_REQ Send event:[9] CMAC ! CMAC_Config_REQ = PDU (view PDU) 00:02:03.530 - Primitive: CMAC_Config_CNF begin "ca_CMAC_CfgCnf" of type CMAC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 8 against 8 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_CfgCnf" of type CMAC_Config_CNF Receive event:[10] CMAC ? CMAC_Config_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 8 ]} Attach:[4] Exit Test Step ts_SS_RACH_CCCH_Cfg
Attach:[5] Enter Test Step ts_CountConfiguredCell( )
| Assignment:[1] tcv_NumCfgCell := 0 Attach:[2] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 0 , frequenc ...
| (view Test Step parameters) Attach:[2] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[3] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 1 , frequenc ...
| (view Test Step parameters) Assignment:[11] tcv_NumCfgCell := 1 Attach:[3] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[4] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 2 , frequenc ...
| (view Test Step parameters) Attach:[4] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[5] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 3 , frequenc ...
| (view Test Step parameters) Attach:[5] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[6] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 4 , frequenc ...
| (view Test Step parameters) Attach:[6] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[7] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 5 , frequenc ...
| (view Test Step parameters) Attach:[7] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[8] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 6 , frequenc ...
| (view Test Step parameters) Attach:[8] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[9] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 7 , frequenc ...
| (view Test Step parameters) Attach:[9] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[5] Exit Test Step ts_CountConfiguredCell
Attach:[15] Enter Test Step ts_SS_RB_BCCH_BCH_Cfg( 3 )
| 00:02:03.530 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:02:03.540 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} Attach:[15] Exit Test Step ts_SS_RB_BCCH_BCH_Cfg
Attach:[16] Enter Test Step ts_SS_RB_PCCH_Cfg( 3 )
| 00:02:03.540 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:02:03.560 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -2 against -2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -2 ]} Attach:[16] Exit Test Step ts_SS_RB_PCCH_Cfg
Attach:[17] Enter Test Step ts_SS_RB0_Cfg( 3 )
| 00:02:03.560 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:02:03.570 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: 0 ]} 00:02:03.570 - Primitive: CRLC_Config_REQ Send event:[3] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:02:03.590 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[4] CRLC ? CRLC_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: 0 ]} Attach:[17] Exit Test Step ts_SS_RB0_Cfg
Attach:[18] Enter Test Step ts_SetCellCfg( 3 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 3 )
| Assignment:[8] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Assignment:[2] cellConfig := cell_NoDPCH Attach:[3] Enter Test Step ts_SaveCellInfo( 3 )
| Assignment:[8] tcv_CellInfoD := (view Assignment) Attach:[3] Exit Test Step ts_SaveCellInfo
Attach:[18] Exit Test Step ts_SetCellCfg
Attach:[47] Exit Test Step ts_SS_CreateCellDCH
Attach:[48] Enter Test Step ts_SendDefSysInfo( 3 )
| Attach:[1] Enter Test Step ts_UTRAN_GERAN_ParaInit( 3 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 3 )
| Assignment:[8] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Assignment:[3] tcv_SIB3 := (view Assignment) Assignment:[3] tcv_SIB4 := (view Assignment) Attach:[1] Exit Test Step ts_UTRAN_GERAN_ParaInit
Attach:[2] Enter Test Step ts_CellDependentPara( 3 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 3 )
| Assignment:[8] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Assignment:[9] cellIdentity := '0000000000000000000000000011'B Assignment:[9] cellIdentity := '0000000000000000000000000011'B Attach:[2] Exit Test Step ts_CellDependentPara
Attach:[3] Enter Test Step ts_InitializeSIB2AndSIB18( { cellId: 3 , frequenc ...
| (view Test Step parameters) Assignment:[1] tcv_SIB2 := { ura_IdentityList: [ '0000000000000010'B ] , nonCriticalExtensions: OMIT} Attach:[5] Enter Test Step ts_InitializeSIB2AndSIB18::lt_Init2PLMN( { cellId: 3 , frequenc ...
| (view Test Step parameters) Assignment:[12] tcv_SIB18 := (view Assignment) Attach:[5] Exit Test Step ts_InitializeSIB2AndSIB18::lt_Init2PLMN
Attach:[3] Exit Test Step ts_InitializeSIB2AndSIB18
Attach:[4] Enter Test Step ts_InitializeSIB11_SIB12( 3 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 3 )
| Assignment:[8] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[5] Enter Test Step ts_InitializeSIB11_SIB12::lt_1Or2PLMN( 3 )
| Assignment:[16] tcv_SIB11 := (view Assignment) Assignment:[16] tcv_SIB12 := (view Assignment) Attach:[5] Exit Test Step ts_InitializeSIB11_SIB12::lt_1Or2PLMN
Attach:[4] Exit Test Step ts_InitializeSIB11_SIB12
Attach:[6] Enter Test Step ts_SendNoSegDefSchedul( 3 )
| Attach:[1] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:02:03.590 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[1] Exit Test Step ts_Scheduling
00:02:03.600 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[2] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} 00:02:03.600 - Primitive: RLC_TR_DATA_REQ 00:02:03.600 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[3] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[6] Exit Test Step ts_SendNoSegDefSchedul
Attach:[7] Enter Test Step ts_SendSIB1( { cn_CommonGSM_MAP_NAS ...
| (view Test Step parameters) Assignment:[1] tcv_SIB1 := (view Assignment) 00:02:03.600 - Primitive: o_SIB_PER_Encoding Assignment:[1] seg1 := (view Assignment) 00:02:03.600 - Primitive: o_SIB_PER_Encoding Assignment:[1] seg2 := '00000000000000000010'B Attach:[4] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:02:03.600 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[4] Exit Test Step ts_Scheduling
00:02:03.620 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[5] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} 00:02:03.620 - Primitive: RLC_TR_DATA_REQ 00:02:03.620 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[6] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Assignment:[7] sysInfoType1 := 5 Attach:[8] Enter Test Step ts_ChangeMIB_ValueTag( )
| Assignment:[2] mib_ValueTag := 4 Assignment:[2] tcv_MIB_ValueTagChanged := GcTRUE Attach:[8] Exit Test Step ts_ChangeMIB_ValueTag
Attach:[7] Exit Test Step ts_SendSIB1
Attach:[8] Enter Test Step ts_SendSIB2( { ura_IdentityList: [ ...
| (view Test Step parameters) Assignment:[1] tcv_SIB2 := { ura_IdentityList: [ '0000000000000010'B ] , nonCriticalExtensions: OMIT} 00:02:03.620 - Primitive: o_SIB_PER_Encoding Assignment:[1] seg1 := '00000000000000000010'B 00:02:03.620 - Primitive: o_SIB_PER_Encoding Assignment:[1] seg2 := (view Assignment) Attach:[4] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:02:03.620 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[4] Exit Test Step ts_Scheduling
00:02:03.630 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[5] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} 00:02:03.630 - Primitive: RLC_TR_DATA_REQ 00:02:03.630 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[6] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Assignment:[7] sysInfoType2 := 4 Attach:[8] Enter Test Step ts_ChangeMIB_ValueTag( )
| Attach:[8] Exit Test Step ts_ChangeMIB_ValueTag
Attach:[8] Exit Test Step ts_SendSIB2
Attach:[9] Enter Test Step ts_SendSIB3( { sib4indicator: GcTRU ...
| (view Test Step parameters) Assignment:[1] tcv_SIB3 := (view Assignment) 00:02:03.630 - Primitive: o_SIB_PER_Encoding Assignment:[1] seg1 := (view Assignment) 00:02:03.630 - Primitive: o_SIB_PER_Encoding Assignment:[1] seg2 := '100000101000000010000001'B Attach:[4] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:02:03.650 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[4] Exit Test Step ts_Scheduling
00:02:03.670 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[5] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} 00:02:03.670 - Primitive: RLC_TR_DATA_REQ 00:02:03.670 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[6] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Assignment:[7] sysInfoType3 := 4 Attach:[8] Enter Test Step ts_ChangeMIB_ValueTag( )
| Attach:[8] Exit Test Step ts_ChangeMIB_ValueTag
Attach:[9] Exit Test Step ts_SendSIB3
Attach:[10] Enter Test Step ts_SendSIB4( { cellIdentity: '00000 ...
| (view Test Step parameters) Assignment:[1] tcv_SIB4 := (view Assignment) 00:02:03.670 - Primitive: o_SIB_PER_Encoding Assignment:[1] seg1 := (view Assignment) 00:02:03.670 - Primitive: o_SIB_PER_Encoding Assignment:[1] seg2 := '100000101000000010000001'B Attach:[4] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:02:03.670 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[4] Exit Test Step ts_Scheduling
00:02:03.680 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[5] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} 00:02:03.680 - Primitive: RLC_TR_DATA_REQ 00:02:03.680 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[6] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Assignment:[7] sysInfoType4 := 4 Attach:[8] Enter Test Step ts_ChangeMIB_ValueTag( )
| Attach:[8] Exit Test Step ts_ChangeMIB_ValueTag
Attach:[10] Exit Test Step ts_SendSIB4
Attach:[11] Enter Test Step ts_SendSIB5( { sib6indicator: GcTRU ...
| (view Test Step parameters) 00:02:03.710 - Primitive: o_SIB_PER_Encoding Assignment:[1] tcv_Segs := (view Assignment) Assignment:[38] sysInfoType5 := 4 Assignment:[38] scheduling := (view Assignment) Attach:[39] Enter Test Step ts_ChangeMIB_ValueTag( )
| Attach:[39] Exit Test Step ts_ChangeMIB_ValueTag
Attach:[40] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:02:03.740 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[40] Exit Test Step ts_Scheduling
00:02:03.760 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[41] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} 00:02:03.760 - Primitive: RLC_TR_DATA_REQ 00:02:03.760 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[42] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[43] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:02:03.760 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[43] Exit Test Step ts_Scheduling
00:02:03.780 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[44] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} 00:02:03.780 - Primitive: RLC_TR_DATA_REQ 00:02:03.780 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[45] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[46] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:02:03.780 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[46] Exit Test Step ts_Scheduling
00:02:03.790 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[47] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} 00:02:03.790 - Primitive: RLC_TR_DATA_REQ 00:02:03.790 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[48] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[49] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:02:03.790 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[49] Exit Test Step ts_Scheduling
00:02:03.810 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[50] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} 00:02:03.810 - Primitive: RLC_TR_DATA_REQ 00:02:03.810 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[52] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[11] Exit Test Step ts_SendSIB5
Attach:[12] Enter Test Step ts_SendSIB6( { pich_PowerOffset: -5 ...
| (view Test Step parameters) 00:02:03.810 - Primitive: o_SIB_PER_Encoding Assignment:[1] tcv_Segs := (view Assignment) Assignment:[5] sysInfoType6 := 4 Assignment:[5] scheduling := { scheduling: { segCount: OMIT, sib_Pos: [rep64: 3 ], sib_PosOffsetInfo: OMIT} } Attach:[6] Enter Test Step ts_ChangeSB1_ValueTag( )
| Assignment:[2] tcv_SB1_ValueTag := 4 Assignment:[2] sysInfoTypeSB1 := 4 Assignment:[2] tcv_SB1_ValueTagChanged := GcTRUE Attach:[3] Enter Test Step ts_ChangeMIB_ValueTag( )
| Attach:[3] Exit Test Step ts_ChangeMIB_ValueTag
Attach:[6] Exit Test Step ts_ChangeSB1_ValueTag
Attach:[7] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:02:03.810 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[7] Exit Test Step ts_Scheduling
00:02:03.820 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[8] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} Attach:[9] Enter Test Step ts_SendSIB6::lt_CompleteSIB( systemInformationBlockType6 )
| 00:02:03.820 - Primitive: RLC_TR_DATA_REQ 00:02:03.820 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[76] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[9] Exit Test Step ts_SendSIB6::lt_CompleteSIB
Attach:[10] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:02:03.820 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[10] Exit Test Step ts_Scheduling
00:02:03.840 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[11] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} 00:02:03.840 - Primitive: RLC_TR_DATA_REQ 00:02:03.840 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[12] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[13] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:02:03.840 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[13] Exit Test Step ts_Scheduling
00:02:03.850 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[14] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} 00:02:03.850 - Primitive: RLC_TR_DATA_REQ 00:02:03.850 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[15] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[16] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:02:03.850 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[16] Exit Test Step ts_Scheduling
00:02:03.870 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[17] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} 00:02:03.870 - Primitive: RLC_TR_DATA_REQ 00:02:03.870 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[18] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[12] Exit Test Step ts_SendSIB6
Attach:[13] Enter Test Step ts_SendSIB7( { modeSpecificInfo: [f ...
| (view Test Step parameters) 00:02:03.870 - Primitive: o_SIB_PER_Encoding Assignment:[1] tcv_Segs := (view Assignment) Assignment:[1] tcv_SIB7 := (view Assignment) Attach:[4] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:02:03.870 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[4] Exit Test Step ts_Scheduling
00:02:03.880 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[5] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} Attach:[6] Enter Test Step ts_SendSIB7::lt_CompleteSIB( systemInformationBlockType7 )
| 00:02:03.880 - Primitive: RLC_TR_DATA_REQ 00:02:03.880 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[13] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[6] Exit Test Step ts_SendSIB7::lt_CompleteSIB
Attach:[7] Enter Test Step ts_SendSIB7::lt_ConcatWithSIB3( { modeSpecificInfo: [f ...
| (view Test Step parameters) 00:02:03.880 - Primitive: o_SIB_PER_Encoding Assignment:[14] seg1 := '100000101000000010000001'B 00:02:03.880 - Primitive: o_SIB_PER_Encoding Assignment:[14] seg2 := (view Assignment) Attach:[17] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:02:03.880 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[17] Exit Test Step ts_Scheduling
00:02:03.900 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[18] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} 00:02:03.900 - Primitive: RLC_TR_DATA_REQ 00:02:03.900 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[19] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[7] Exit Test Step ts_SendSIB7::lt_ConcatWithSIB3
Attach:[8] Enter Test Step ts_SendSIB7::lt_ConcatWithSIB18( { modeSpecificInfo: [f ...
| (view Test Step parameters) 00:02:03.900 - Primitive: o_SIB_PER_Encoding Assignment:[20] seg2 := '100010000001000000000001000000001'B Attach:[23] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:02:03.900 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[23] Exit Test Step ts_Scheduling
00:02:03.920 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[24] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} 00:02:03.920 - Primitive: RLC_TR_DATA_REQ 00:02:03.920 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[25] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[8] Exit Test Step ts_SendSIB7::lt_ConcatWithSIB18
Attach:[9] Enter Test Step ts_SendSIB7::lt_ConcatWithSIB4( { modeSpecificInfo: [f ...
| (view Test Step parameters) 00:02:03.920 - Primitive: o_SIB_PER_Encoding Assignment:[26] seg2 := (view Assignment) Attach:[29] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:02:03.920 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[29] Exit Test Step ts_Scheduling
00:02:03.930 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[30] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} 00:02:03.930 - Primitive: RLC_TR_DATA_REQ 00:02:03.930 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[31] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[9] Exit Test Step ts_SendSIB7::lt_ConcatWithSIB4
Attach:[13] Exit Test Step ts_SendSIB7
Attach:[14] Enter Test Step ts_SendSIB11( { sib12indicator: GcTR ...
| (view Test Step parameters) 00:02:03.950 - Primitive: o_SIB_PER_Encoding Assignment:[1] tcv_Segs := (view Assignment) Assignment:[17] sysInfoType11 := 4 Assignment:[17] scheduling := (view Assignment) Attach:[18] Enter Test Step ts_ChangeSB1_ValueTag( )
| Attach:[18] Exit Test Step ts_ChangeSB1_ValueTag
Attach:[19] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:02:04.010 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[19] Exit Test Step ts_Scheduling
00:02:04.030 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[20] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} 00:02:04.030 - Primitive: RLC_TR_DATA_REQ 00:02:04.030 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[21] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[22] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:02:04.030 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[22] Exit Test Step ts_Scheduling
00:02:04.040 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[23] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} 00:02:04.040 - Primitive: RLC_TR_DATA_REQ 00:02:04.040 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[24] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[25] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:02:04.040 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[25] Exit Test Step ts_Scheduling
00:02:04.060 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[26] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} 00:02:04.060 - Primitive: RLC_TR_DATA_REQ 00:02:04.060 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[28] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[14] Exit Test Step ts_SendSIB11
Attach:[15] Enter Test Step ts_SendSIB12( { fach_MeasurementOcca ...
| (view Test Step parameters) 00:02:04.060 - Primitive: o_SIB_PER_Encoding Assignment:[1] tcv_Segs := (view Assignment) Assignment:[5] sysInfoType12 := 4 Assignment:[5] scheduling := { scheduling: { segCount: OMIT, sib_Pos: [rep64: 13 ], sib_PosOffsetInfo: OMIT} } Attach:[6] Enter Test Step ts_ChangeSB1_ValueTag( )
| Attach:[6] Exit Test Step ts_ChangeSB1_ValueTag
Attach:[7] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:02:04.060 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[7] Exit Test Step ts_Scheduling
00:02:04.070 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[8] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} Attach:[9] Enter Test Step ts_SendSIB12::lt_CompleteSIB( systemInformationBlockType12 )
| 00:02:04.070 - Primitive: RLC_TR_DATA_REQ 00:02:04.070 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[50] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[9] Exit Test Step ts_SendSIB12::lt_CompleteSIB
Attach:[10] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:02:04.070 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[10] Exit Test Step ts_Scheduling
00:02:04.090 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[11] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} 00:02:04.090 - Primitive: RLC_TR_DATA_REQ 00:02:04.090 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[12] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[13] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:02:04.090 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[13] Exit Test Step ts_Scheduling
00:02:04.100 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[14] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} 00:02:04.100 - Primitive: RLC_TR_DATA_REQ 00:02:04.100 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[15] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[15] Exit Test Step ts_SendSIB12
Attach:[16] Enter Test Step ts_SendSIB18( { idleModePLMNIdentiti ...
| (view Test Step parameters) Assignment:[1] tcv_SIB18 := (view Assignment) 00:02:04.100 - Primitive: o_SIB_PER_Encoding Assignment:[1] seg1 := '100010000001000000000001000000001'B 00:02:04.100 - Primitive: o_SIB_PER_Encoding Assignment:[1] seg2 := '100000101000000010000001'B Attach:[4] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:02:04.100 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[4] Exit Test Step ts_Scheduling
00:02:04.120 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[5] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} 00:02:04.120 - Primitive: RLC_TR_DATA_REQ 00:02:04.120 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[6] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Assignment:[7] sysInfoType18 := 4 Attach:[8] Enter Test Step ts_ChangeSB1_ValueTag( )
| Attach:[8] Exit Test Step ts_ChangeSB1_ValueTag
Attach:[16] Exit Test Step ts_SendSIB18
Attach:[17] Enter Test Step ts_SendSB1_DefSchedul( { sib_ReferenceList: [ ...
| (view Test Step parameters) 00:02:04.120 - Primitive: o_SIB_PER_Encoding Assignment:[1] tcv_Segs := (view Assignment) Attach:[3] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:02:04.120 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[3] Exit Test Step ts_Scheduling
00:02:04.130 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[4] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} Attach:[5] Enter Test Step ts_SendSB1_DefSchedul::lt_CompleteSIB( schedulingBlock1 )
| 00:02:04.130 - Primitive: RLC_TR_DATA_REQ 00:02:04.130 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[12] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[5] Exit Test Step ts_SendSB1_DefSchedul::lt_CompleteSIB
Attach:[6] Enter Test Step ts_ChangeSB1_ValueTag( )
| Attach:[6] Exit Test Step ts_ChangeSB1_ValueTag
Assignment:[7] scheduling := { scheduling: { segCount: OMIT, sib_Pos: [rep16: 1 ], sib_PosOffsetInfo: OMIT} } Assignment:[7] tcv_SB1_ValueTagChanged := GcFALSE Attach:[17] Exit Test Step ts_SendSB1_DefSchedul
Attach:[18] Enter Test Step ts_SendMIB( { mib_ValueTag: 4 , pl ...
| (view Test Step parameters) Attach:[1] Enter Test Step ts_SetTmpCellInfo( 3 )
| Assignment:[8] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Assignment:[2] mcc := [ 0 , 0 , 2 ] Assignment:[2] mnc := [ 0 , 1 ] 00:02:04.130 - Primitive: o_SIB_PER_Encoding Assignment:[3] tcv_Segs := (view Assignment) Attach:[6] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:02:04.170 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[6] Exit Test Step ts_Scheduling
00:02:04.180 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[7] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} Attach:[8] Enter Test Step ts_SendMIB::lt_CompleteSIB( masterInformationBlock )
| 00:02:04.180 - Primitive: RLC_TR_DATA_REQ 00:02:04.180 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[13] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[8] Exit Test Step ts_SendMIB::lt_CompleteSIB
Assignment:[9] tcv_MIB_ValueTagChanged := GcFALSE Attach:[18] Exit Test Step ts_SendMIB
Attach:[48] Exit Test Step ts_SendDefSysInfo
Attach:[21] Exit Test Step tc_12_4_1_2::lt_ActivateCellD_Step12
Attach:[22] Enter Test Step ts_VerifyNoAccess( 30 )
| StartTimer:[3] t_WaitS [15] 30 s Timed out Timer:t_WaitS TimeOut:[5] t_WaitS [15] 30 s Preliminary verdict:[5] (PASS) Attach:[22] Exit Test Step ts_VerifyNoAccess
Attach:[23] Enter Test Step ts_MM_PwrOrUSIM_Off( GcTRUE )
| Attach:[4] Enter Test Step ts_MMI_UE_SwitchOff( )
| 00:02:34.200 - Primitive: MMI_CmdReq Send event:[2] Ut ! MMI_CmdReq = PDU: { cmd: "Please switch off the UE" } 00:02:37.480 - Primitive: MMI_CmdCnf begin "ca_MMI_CmdCnf" of type MMI_CmdCnf (SEQUENCE) [UNIVERSAL 16] begin "result" of type BOOLEAN [UNIVERSAL 1] matching GcTRUE against GcTRUE end "result" of type BOOLEAN end "ca_MMI_CmdCnf" of type MMI_CmdCnf Receive event:[3] Ut ? MMI_CmdCnf = PDU: { result: GcTRUE , resultString: OMIT} Assignment:[4] tcv_UE_SwitchedOn := GcFALSE Attach:[4] Exit Test Step ts_MMI_UE_SwitchOff
Attach:[23] Exit Test Step ts_MM_PwrOrUSIM_Off
Attach:[24] Enter Test Step ts_MM_PwrOrUSIM_On( GcTRUE )
| Attach:[4] Enter Test Step ts_MMI_UE_SwitchOn( )
| 00:02:37.480 - Primitive: MMI_CmdReq Send event:[2] Ut ! MMI_CmdReq = PDU: { cmd: "Please switch on the UE" } 00:02:53.230 - Primitive: MMI_CmdCnf begin "ca_MMI_CmdCnf" of type MMI_CmdCnf (SEQUENCE) [UNIVERSAL 16] begin "result" of type BOOLEAN [UNIVERSAL 1] matching GcTRUE against GcTRUE end "result" of type BOOLEAN end "ca_MMI_CmdCnf" of type MMI_CmdCnf Receive event:[3] Ut ? MMI_CmdCnf = PDU: { result: GcTRUE , resultString: OMIT} Assignment:[4] tcv_UE_SwitchedOn := GcTRUE Attach:[4] Exit Test Step ts_MMI_UE_SwitchOn
Attach:[24] Exit Test Step ts_MM_PwrOrUSIM_On
Attach:[25] Enter Test Step tc_12_4_1_2::lt_Attach_Steps_17To19( )
| Assignment:[37] tcv_PS_KeySeq := '111'B Attach:[38] Enter Test Step ts_MM_RegistrationHandleAttachReqIMSI( 3 )
| Assignment:[2] tcv_GMM_AttachExpect := GcTRUE Assignment:[2] tcv_GMM_AttachRec := GcFALSE Attach:[3] Enter Test Step ts_RRC_ConnEst( 3 )
| Attach:[1] Enter Test Step ts_SS_PrepareCellRRC_ConnEst( 3 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 3 )
| Assignment:[8] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[4] Enter Test Step ts_SS_PrepareCellRRC_ConnEst::lt_ReconfOldDPCH_Cell( 3 )
| Attach:[42] Enter Test Step ts_SS_RelDPCH( 1 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 1 )
| Assignment:[4] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[3] Enter Test Step ts_SS_RelDPCH::lt_RelSRB1_4( 1 )
| Attach:[119] Enter Test Step ts_CRLC_Rel( -1 )
| 00:02:53.230 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:02:53.240 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 1 ]} Attach:[119] Exit Test Step ts_CRLC_Rel
Attach:[120] Enter Test Step ts_CRLC_Rel( -1 )
| 00:02:53.240 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:02:53.260 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 2 ]} Attach:[120] Exit Test Step ts_CRLC_Rel
Attach:[121] Enter Test Step ts_CRLC_Rel( -1 )
| 00:02:53.260 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:02:53.280 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 3 ]} Attach:[121] Exit Test Step ts_CRLC_Rel
Attach:[122] Enter Test Step ts_CRLC_Rel( -1 )
| 00:02:53.280 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:02:53.290 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 4 ]} Attach:[122] Exit Test Step ts_CRLC_Rel
Attach:[3] Exit Test Step ts_SS_RelDPCH::lt_RelSRB1_4
Attach:[4] Enter Test Step ts_CMAC_Rel( -1 )
| 00:02:53.290 - Primitive: CMAC_Config_REQ Send event:[1] CMAC ! CMAC_Config_REQ = PDU (view PDU) 00:02:53.320 - Primitive: CMAC_Config_CNF begin "ca_CMAC_CfgCnf" of type CMAC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 26 against 26 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_CfgCnf" of type CMAC_Config_CNF Receive event:[2] CMAC ? CMAC_Config_CNF = PDU: { cellId: -1 , routingInfo: [physicalChannelIdentity: 26 ]} Attach:[4] Exit Test Step ts_CMAC_Rel
Attach:[5] Enter Test Step ts_CMAC_Rel( -1 )
| 00:02:53.320 - Primitive: CMAC_Config_REQ Send event:[1] CMAC ! CMAC_Config_REQ = PDU (view PDU) 00:02:53.350 - Primitive: CMAC_Config_CNF begin "ca_CMAC_CfgCnf" of type CMAC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 20 against 20 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_CfgCnf" of type CMAC_Config_CNF Receive event:[2] CMAC ? CMAC_Config_CNF = PDU: { cellId: -1 , routingInfo: [physicalChannelIdentity: 20 ]} Attach:[5] Exit Test Step ts_CMAC_Rel
Attach:[6] Enter Test Step ts_CPHY_TrChRelDCH_NoSHO( 1 )
| 00:02:53.350 - Primitive: CPHY_TrCH_Release_REQ Send event:[1] CPHY ! CPHY_TrCH_Release_REQ = PDU (view PDU) 00:02:53.370 - Primitive: CPHY_TrCH_Release_CNF begin "ca_PHY_RelCnf" of type CPHY_TrCH_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 26 against 26 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_PHY_RelCnf" of type CPHY_TrCH_Release_CNF Receive event:[2] CPHY ? CPHY_TrCH_Release_CNF = PDU (view PDU) Attach:[6] Exit Test Step ts_CPHY_TrChRelDCH_NoSHO
Attach:[7] Enter Test Step ts_CPHY_TrChRelDCH_NoSHO( 1 )
| 00:02:53.370 - Primitive: CPHY_TrCH_Release_REQ Send event:[1] CPHY ! CPHY_TrCH_Release_REQ = PDU (view PDU) 00:02:53.380 - Primitive: CPHY_TrCH_Release_CNF begin "ca_PHY_RelCnf" of type CPHY_TrCH_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 20 against 20 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_PHY_RelCnf" of type CPHY_TrCH_Release_CNF Receive event:[2] CPHY ? CPHY_TrCH_Release_CNF = PDU (view PDU) Attach:[7] Exit Test Step ts_CPHY_TrChRelDCH_NoSHO
Attach:[8] Enter Test Step ts_SS_StopRL( 1 )
| 00:02:53.380 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 1 , routingInfo: [physicalChannelIdentity: 26 ]} 00:02:53.400 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 26 against 26 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 1 , routingInfo: [physicalChannelIdentity: 26 ]} Attach:[8] Exit Test Step ts_SS_StopRL
Attach:[9] Enter Test Step ts_SS_StopRL( 1 )
| 00:02:53.400 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 1 , routingInfo: [physicalChannelIdentity: 20 ]} 00:02:53.420 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 20 against 20 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 1 , routingInfo: [physicalChannelIdentity: 20 ]} Attach:[9] Exit Test Step ts_SS_StopRL
Attach:[42] Exit Test Step ts_SS_RelDPCH
Assignment:[43] cellConfig := cell_NoDPCH Assignment:[43] DL_DPCH_SHO := GcFALSE Assignment:[43] UL_DPCH_SHO := GcFALSE Attach:[4] Exit Test Step ts_SS_PrepareCellRRC_ConnEst::lt_ReconfOldDPCH_Cell
Attach:[5] Enter Test Step ts_SS_AddDPCH( 3 )
| Attach:[1] Enter Test Step ts_SS_1DCH_DCCH_Cfg( 3 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 3 )
| Assignment:[8] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Assignment:[3] tcv_TGCFN := 0 00:02:53.420 - Primitive: CPHY_RL_Setup_REQ Send event:[4] CPHY ! CPHY_RL_Setup_REQ = PDU (view PDU) 00:02:53.430 - Primitive: CPHY_RL_Setup_CNF begin "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 26 against 26 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF Receive event:[5] CPHY ? CPHY_RL_Setup_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 26 ]} 00:02:53.430 - Primitive: CPHY_TrCH_Config_REQ Send event:[6] CPHY ! CPHY_TrCH_Config_REQ = PDU (view PDU) 00:02:53.460 - Primitive: CPHY_TrCH_Config_CNF begin "ca_TrChCfgCnf" of type CPHY_TrCH_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 26 against 26 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_TrChCfgCnf" of type CPHY_TrCH_Config_CNF Receive event:[7] CPHY ? CPHY_TrCH_Config_CNF = PDU (view PDU) 00:02:53.460 - Primitive: CMAC_Config_REQ Send event:[8] CMAC ! CMAC_Config_REQ = PDU (view PDU) 00:02:53.510 - Primitive: CMAC_Config_CNF begin "ca_CMAC_CfgCnf" of type CMAC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 26 against 26 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_CfgCnf" of type CMAC_Config_CNF Receive event:[9] CMAC ? CMAC_Config_CNF = PDU: { cellId: -1 , routingInfo: [physicalChannelIdentity: 26 ]} 00:02:53.510 - Primitive: CPHY_RL_Setup_REQ Send event:[10] CPHY ! CPHY_RL_Setup_REQ = PDU (view PDU) 00:02:53.530 - Primitive: CPHY_RL_Setup_CNF begin "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 20 against 20 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF Receive event:[11] CPHY ? CPHY_RL_Setup_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 20 ]} 00:02:53.530 - Primitive: CPHY_TrCH_Config_REQ Send event:[12] CPHY ! CPHY_TrCH_Config_REQ = PDU (view PDU) 00:02:53.570 - Primitive: CPHY_TrCH_Config_CNF begin "ca_TrChCfgCnf" of type CPHY_TrCH_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 20 against 20 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_TrChCfgCnf" of type CPHY_TrCH_Config_CNF Receive event:[13] CPHY ? CPHY_TrCH_Config_CNF = PDU (view PDU) 00:02:53.570 - Primitive: CMAC_Config_REQ Send event:[14] CMAC ! CMAC_Config_REQ = PDU (view PDU) 00:02:53.600 - Primitive: CMAC_Config_CNF begin "ca_CMAC_CfgCnf" of type CMAC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 20 against 20 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_CfgCnf" of type CMAC_Config_CNF Receive event:[15] CMAC ? CMAC_Config_CNF = PDU: { cellId: -1 , routingInfo: [physicalChannelIdentity: 20 ]} Attach:[1] Exit Test Step ts_SS_1DCH_DCCH_Cfg
Attach:[2] Enter Test Step ts_SS_RB1_ToRB4_Cfg( )
| 00:02:53.600 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:02:53.620 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 1 ]} 00:02:53.620 - Primitive: CRLC_Config_REQ Send event:[3] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:02:53.630 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[4] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 2 ]} 00:02:53.630 - Primitive: CRLC_Config_REQ Send event:[5] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:02:53.650 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[6] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 3 ]} 00:02:53.650 - Primitive: CRLC_Config_REQ Send event:[7] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:02:53.670 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[8] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 4 ]} Attach:[2] Exit Test Step ts_SS_RB1_ToRB4_Cfg
Attach:[5] Exit Test Step ts_SS_AddDPCH
Assignment:[6] cellConfig := cell_DCH_StandAloneSRB_NoConn Assignment:[6] DL_DPCH_SHO := GcTRUE Assignment:[6] UL_DPCH_SHO := GcTRUE Attach:[7] Enter Test Step ts_SaveCellInfo( 3 )
| Assignment:[8] tcv_CellInfoD := (view Assignment) Attach:[7] Exit Test Step ts_SaveCellInfo
Attach:[1] Exit Test Step ts_SS_PrepareCellRRC_ConnEst
Attach:[2] Enter Test Step ts_SetTmpCellInfo( 3 )
| Assignment:[8] tcv_TmpCellInfo := (view Assignment) Attach:[2] Exit Test Step ts_SetTmpCellInfo
Attach:[3] Enter Test Step ts_RRC_ConnEst::lt_RcvConnReq( 3 )
| 00:03:27.090 - Primitive: RLC_TR_DATA_IND: rrcConnectionRequest 00:03:27.090 - Primitive: RLC_TR_DATA_IND begin "car_RRC_ConnReq" of type RLC_TR_DATA_IND (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "tM_message" of type CHOICE [UNIVERSAL 31] begin "uL_CCCH_Message" of type UL_CCCH_Message (SEQUENCE) [UNIVERSAL 16] begin "message" of type UL_CCCH_MessageType (CHOICE) [UNIVERSAL 31] begin "rrcConnectionRequest" of type RRCConnectionRequest (SEQUENCE) [UNIVERSAL 16] begin "initialUE_Identity" of type InitialUE_Identity (CHOICE) [UNIVERSAL 31] begin InitialUE_Identity (CHOICE) [UNIVERSAL 31] begin "imsi" of type IMSI_GSM_MAP (SEQUENCEOF) [UNIVERSAL 28] matching [ 0 , 0 , 1 , 0 , 1 , 0 , 0 , 0 , 0 , 0 , 0 , 0 , 3 , 3 , 3 ] against ? end "imsi" of type IMSI_GSM_MAP end InitialUE_Identity matching [imsi: [ 0 , 0 , 1 , 0 , 1 , 0 , 0 , 0 , 0 , 0 , 0 , 0 , 3 , 3 , 3 ] ] against ([imsi: ?], [tmsi_and_LAI: ?], [p_TMSI_and_RAI: ?], [imei: ?]) end "initialUE_Identity" of type InitialUE_Identity begin "establishmentCause" of type EstablishmentCause (ENUMERATED) [UNIVERSAL 10] matching registration against registration end "establishmentCause" of type EstablishmentCause begin "protocolErrorIndicator" of type ProtocolErrorIndicator (ENUMERATED) [UNIVERSAL 10] matching noError against noError end "protocolErrorIndicator" of type ProtocolErrorIndicator end "rrcConnectionRequest" of type RRCConnectionRequest end "message" of type UL_CCCH_MessageType end "uL_CCCH_Message" of type UL_CCCH_Message end "tM_message" of type CHOICE end "car_RRC_ConnReq" of type RLC_TR_DATA_IND Assignment:[7] tcv_InitialUE_Id := [imsi: [ 0 , 0 , 1 , 0 , 1 , 0 , 0 , 0 , 0 , 0 , 0 , 0 , 3 , 3 , 3 ] ] Receive event:[7] TM ? RLC_TR_DATA_IND = PDU (view PDU) Attach:[3] Exit Test Step ts_RRC_ConnEst::lt_RcvConnReq
Attach:[4] Enter Test Step ts_RRC_ConnEst::lt_Send_ConnSetUp( 3 )
| 00:03:27.090 - Primitive: RLC_UM_DATA_REQ 00:03:27.090 - Primitive: RLC_UM_DATA_REQ: rrcConnectionSetup Send event:[31] UM ! RLC_UM_DATA_REQ = PDU (view PDU) Attach:[33] Enter Test Step ts_SetCellCfg( 3 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 3 )
| Assignment:[8] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Assignment:[2] cellConfig := cell_DCH_StandAloneSRB Attach:[3] Enter Test Step ts_SaveCellInfo( 3 )
| Assignment:[8] tcv_CellInfoD := (view Assignment) Attach:[3] Exit Test Step ts_SaveCellInfo
Attach:[33] Exit Test Step ts_SetCellCfg
Attach:[4] Exit Test Step ts_RRC_ConnEst::lt_Send_ConnSetUp
Attach:[5] Enter Test Step ts_RRC_ReceiveConnSetupCmpl( 3 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 3 )
| Assignment:[8] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
StartTimer:[3] t_WaitMS [13500] 13500 ms 00:03:27.570 - Primitive: RLC_AM_DATA_IND: rrcConnectionSetupComplete 00:03:27.570 - Primitive: RLC_AM_DATA_IND begin "car_RRC_ConnSetupCmpl" of type RLC_AM_DATA_IND (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "integrityResult" of type IntegrityResult (CHOICE) [UNIVERSAL 31] matching [integrityUsed: i_pass] against ? end "integrityResult" of type IntegrityResult begin "aM_message" of type CHOICE [UNIVERSAL 31] begin "uL_DCCH_Message" of type UL_DCCH_Message (SEQUENCE) [UNIVERSAL 16] begin "message" of type UL_DCCH_MessageType (CHOICE) [UNIVERSAL 31] begin "rrcConnectionSetupComplete" of type RRCConnectionSetupComplete (SEQUENCE) [UNIVERSAL 16] begin "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier (INTEGER) [UNIVERSAL 2] matching 0 against 0 end "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier begin "startList" of type STARTList (SEQUENCEOF) [UNIVERSAL 28] matching [ { cn_DomainIdentity: ps_domain, start_Value: '00000000000000000010'B } , { cn_DomainIdentity: cs_domain, start_Value: '00000000000000000010'B } ] against ? end "startList" of type STARTList begin "ue_RadioAccessCapability" of type UE_RadioAccessCapability (SEQUENCE) [UNIVERSAL 16] matching { accessStratumReleaseIndicator: r99, pdcp_Capability: { losslessSRNS_RelocationSupport: GcFALSE , supportForRfc2507: [notSupported: NULL]} , rlc_Capability: { totalRLC_AM_BufferSize: kb50, maximumRLC_WindowSize: mws2047, maximumAM_EntityNumber: am6} , transportChannelCapability: { dl_TransChCapability: { maxNoBitsReceived: b8960, maxConvCodeBitsReceived: b1280, turboDecodingSupport: [supported: b8960], maxSimultaneousTransChs: e8, maxSimultaneousCCTrCH_Count: 1 , maxReceivedTransportBlocks: tb32, maxNumberOfTFC: tfc128, maxNumberOfTF: tf64} , ul_TransChCapability: { maxNoBitsTransmitted: b3840, maxConvCodeBitsTransmitted: b1280, turboEncodingSupport: [supported: b3840], maxSimultaneousTransChs: e8, modeSpecificInfo: [fdd: NULL], maxTransmittedBlocks: tb32, maxNumberOfTFC: tfc64, maxNumberOfTF: tf32} } , rf_Capability: { fddRF_Capability: { ue_PowerClass: 4 , txRxFrequencySeparation: mhz190} , tddRF_Capability: OMIT} , physicalChannelCapability: { fddPhysChCapability: { downlinkPhysChCapability: { maxNoDPCH_PDSCH_Codes: 1 , maxNoPhysChBitsReceived: b9600, supportForSF_512: GcFALSE , supportOfPDSCH: GcFALSE , simultaneousSCCPCH_DPCH_Reception: [notSupported: NULL]} , uplinkPhysChCapability: { maxNoDPDCH_BitsTransmitted: b4800, supportOfPCPCH: GcFALSE } } , tddPhysChCapability: OMIT} , ue_MultiModeRAT_Capability: { multiRAT_CapabilityList: { supportOfGSM: GcFALSE , supportOfMulticarrier: GcFALSE } , multiModeCapability: fdd} , securityCapability: { cipheringAlgorithmCap: '0000000000000011'B , integrityProtectionAlgorithmCap: '0000000000000010'B } , ue_positioning_Capability: { standaloneLocMethodsSupported: GcFALSE , ue_BasedOTDOA_Supported: GcFALSE , networkAssistedGPS_Supported: noNetworkAssistedGPS, supportForUE_GPS_TimingOfCellFrames: GcFALSE , supportForIPDL: GcFALSE } , measurementCapability: { downlinkCompressedMode: { fdd_Measurements: GcTRUE , tdd_Measurements: OMIT, gsm_Measurements: { gsm900: GcTRUE , dcs1800: GcTRUE , gsm1900: GcTRUE } , multiCarrierMeasurements: GcFALSE } , uplinkCompressedMode: { fdd_Measurements: GcTRUE , tdd_Measurements: OMIT, gsm_Measurements: { gsm900: GcTRUE , dcs1800: GcTRUE , gsm1900: GcTRUE } , multiCarrierMeasurements: GcFALSE } } } against * end "ue_RadioAccessCapability" of type UE_RadioAccessCapability end "rrcConnectionSetupComplete" of type RRCConnectionSetupComplete end "message" of type UL_DCCH_MessageType end "uL_DCCH_Message" of type UL_DCCH_Message end "aM_message" of type CHOICE end "car_RRC_ConnSetupCmpl" of type RLC_AM_DATA_IND Assignment:TSP1: [5] tcv_StartList := (view Assignment) Assignment:TSP1: [5] cipheringAlgorithmCapability := '0000000000000011'B CancelTimer:TSP1: [5] t_WaitMS [13500] 13500 ms Receive event:TSP1: [5] AM ? RLC_AM_DATA_IND = PDU (view PDU) Preliminary verdict:TSP1: [5] (PASS) Attach:[6] Enter Test Step ts_RRC_ReceiveConnSetupCmpl::lt_GetHFN( 3 )
| Assignment:[13] tcv_Count := 2 Attach:[17] Enter Test Step ts_RRC_ReceiveConnSetupCmpl::lt_FirstValue( 3 )
| Assignment:[23] start_PS := '00000000000000000010'B Attach:[17] Exit Test Step ts_RRC_ReceiveConnSetupCmpl::lt_FirstValue
Attach:[18] Enter Test Step ts_RRC_ReceiveConnSetupCmpl::lt_SecondValue( 3 )
| Assignment:[26] start_CS := '00000000000000000010'B Attach:[18] Exit Test Step ts_RRC_ReceiveConnSetupCmpl::lt_SecondValue
Attach:[6] Exit Test Step ts_RRC_ReceiveConnSetupCmpl::lt_GetHFN
Attach:[5] Exit Test Step ts_RRC_ReceiveConnSetupCmpl
Attach:[3] Exit Test Step ts_RRC_ConnEst
Attach:[4] Enter Test Step ts_RegistrationOnCS( 3 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 3 )
| Assignment:[8] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
00:03:27.580 - Primitive: RLC_AM_DATA_IND: initialDirectTransfer 00:03:27.580 - Primitive: RRC_DATA_IND: mm:locationUpdatingRequest begin "car_InitDirectTransfer" of type RRC_DataInd (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "rB_Id" of type SS_RB_Identity (INTEGER) [UNIVERSAL 2] matching 3 against 3 end "rB_Id" of type SS_RB_Identity begin "cN_Domain" of type SS_CN_DomainIdentity (INTEGER) [UNIVERSAL 2] matching 0 against 0 end "cN_Domain" of type SS_CN_DomainIdentity begin "start" of type START_Value (BITSTRING) [UNIVERSAL 3] matching '00000000000000000010'B against ? end "start" of type START_Value begin "msg" of type LOCATIONUPDATINGREQUEST (SEQUENCE) [UNIVERSAL 16] begin "skipIndicator" of type SkipIndicator (BITSTRING) [UNIVERSAL 3] matching '0000'B against '0000'B end "skipIndicator" of type SkipIndicator begin "mMProtocolDiscriminator" of type ProtocolDiscriminator (BITSTRING) [UNIVERSAL 3] matching '0101'B against '0101'B end "mMProtocolDiscriminator" of type ProtocolDiscriminator begin "msgType" of type MsgType (BITSTRING) [UNIVERSAL 3] matching '00001000'B against '??001000'B end "msgType" of type MsgType begin "ciphKeySeqNum" of type CiphKeySeqNum (SEQUENCE) [UNIVERSAL 16] begin "spare1" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against '0'B end "spare1" of type B1 begin "keySeq" of type KeySeq (BITSTRING) [UNIVERSAL 3] matching '111'B against ? end "keySeq" of type KeySeq end "ciphKeySeqNum" of type CiphKeySeqNum begin "locUpdType" of type LocUpdType (SEQUENCE) [UNIVERSAL 16] begin "fOR" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against ? end "fOR" of type B1 begin "spare1" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against '0'B end "spare1" of type B1 begin "lUT" of type B2 (BITSTRING) [UNIVERSAL 3] matching '00'B against ? end "lUT" of type B2 end "locUpdType" of type LocUpdType begin "locAreaId" of type LocAreaId_v (SEQUENCE) [UNIVERSAL 16] begin "plmn" of type OCTETSTRING [UNIVERSAL 4] matching '00F110'O against ? end "plmn" of type OCTETSTRING begin "lac" of type OCTETSTRING [UNIVERSAL 4] matching 'FFFE'O against ? end "lac" of type OCTETSTRING end "locAreaId" of type LocAreaId_v begin "mSClsmk1" of type MS_Clsmk1 (SEQUENCE) [UNIVERSAL 16] begin "spare1" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against '0'B end "spare1" of type B1 begin "revLvl" of type B2 (BITSTRING) [UNIVERSAL 3] matching '10'B against ? end "revLvl" of type B2 begin "eSIND" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against ? end "eSIND" of type B1 begin "a5_1" of type B1 (BITSTRING) [UNIVERSAL 3] matching '1'B against ? end "a5_1" of type B1 begin "rFPwrCap" of type B3 (BITSTRING) [UNIVERSAL 3] matching '111'B against ? end "rFPwrCap" of type B3 end "mSClsmk1" of type MS_Clsmk1 begin "mobileId" of type MS_Identity_lv (SEQUENCE) [UNIVERSAL 16] begin "iel" of type Length (OCTETSTRING) [UNIVERSAL 4] matching '08'O against ? end "iel" of type Length begin "iDigit1" of type B4 (BITSTRING) [UNIVERSAL 3] matching '0000'B against ? end "iDigit1" of type B4 begin "oddEvenInd" of type B1 (BITSTRING) [UNIVERSAL 3] matching '1'B against ? end "oddEvenInd" of type B1 begin "typeOfId" of type B3 (BITSTRING) [UNIVERSAL 3] matching '001'B against ? end "typeOfId" of type B3 begin "otherDigits" of type OCTETSTRING [UNIVERSAL 4] matching '10100000003033'O against ? end "otherDigits" of type OCTETSTRING end "mobileId" of type MS_Identity_lv begin "mSClsmk2" of type MS_Clsmk2 (SEQUENCE) [UNIVERSAL 16] begin "iei" of type IEI8 (BITSTRING) [UNIVERSAL 3] matching '00110011'B against '00110011'B end "iei" of type IEI8 begin "iel" of type Length (OCTETSTRING) [UNIVERSAL 4] matching '03'O against '03'O end "iel" of type Length begin "spare1_1" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against '0'B end "spare1_1" of type B1 begin "revLvl" of type B2 (BITSTRING) [UNIVERSAL 3] matching '10'B against ? end "revLvl" of type B2 begin "eSIND" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against ? end "eSIND" of type B1 begin "a5_1" of type B1 (BITSTRING) [UNIVERSAL 3] matching '1'B against ? end "a5_1" of type B1 begin "rFPwrCap" of type B3 (BITSTRING) [UNIVERSAL 3] matching '111'B against ? end "rFPwrCap" of type B3 begin "spare1_2" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against '0'B end "spare1_2" of type B1 begin "pSCap" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against ? end "pSCap" of type B1 begin "sSSI" of type B2 (BITSTRING) [UNIVERSAL 3] matching '01'B against ? end "sSSI" of type B2 begin "sMCap" of type B1 (BITSTRING) [UNIVERSAL 3] matching '1'B against ? end "sMCap" of type B1 begin "vBS" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against ? end "vBS" of type B1 begin "vGCS" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against ? end "vGCS" of type B1 begin "fC" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against ? end "fC" of type B1 begin "cM3" of type B1 (BITSTRING) [UNIVERSAL 3] matching '1'B against ? end "cM3" of type B1 begin "spare1_3" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against '0'B end "spare1_3" of type B1 begin "lCSVA" of type B1 (BITSTRING) [UNIVERSAL 3] matching '1'B against ? end "lCSVA" of type B1 begin "uCS2" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against ? end "uCS2" of type B1 begin "soLSA" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against ? end "soLSA" of type B1 begin "cMSP" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against ? end "cMSP" of type B1 begin "a5_3" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against ? end "a5_3" of type B1 begin "a5_2" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against ? end "a5_2" of type B1 end "mSClsmk2" of type MS_Clsmk2 end "msg" of type LOCATIONUPDATINGREQUEST end "car_InitDirectTransfer" of type RRC_DataInd Assignment:[2] tcv_Start := '00000000000000000010'B Receive event:[2] Dc ? RRC_DataInd = PDU (view PDU) Attach:[3] Enter Test Step ts_SS_SecurityDownloadStart( cs_domain )
| Assignment:[2] start_CS := '00000000000000000010'B Attach:[3] Exit Test Step ts_SS_SecurityDownloadStart
Attach:[4] Enter Test Step ts_MM_Authentication( 3 )
| Attach:[1] Enter Test Step ts_MM_AuthenticationInit( )
| Attach:[1] Enter Test Step ts_MM_AuthenticationInit::lt_IncrementCiphKeySeqNum( )
| Assignment:[6] tcv_CS_KeySeq := '001'B Attach:[1] Exit Test Step ts_MM_AuthenticationInit::lt_IncrementCiphKeySeqNum
Attach:[2] Enter Test Step ts_MM_AuthenticationInit::lt_AuthCalcAUTN( )
| Assignment:[19] tcv_AuthXDOUT := (view Assignment) Assignment:[20] tcv_AuthCDOUT := '0000000000000000000000000000000000000000000000000000000000000000'B Assignment:[21] tcv_AuthXDOUT_Half := '0101010101000100011101110110011000010001000000000011001100100010'B Assignment:[22] tcv_AuthAK := '011001100001000100000000001100110010001011011101'B Assignment:[23] tcv_AuthAUTN_1 := '011001100001000100000000001100110010001011011101'B Assignment:[24] tcv_AuthMAC := '0101010101000100011101110110011000010001000000000011001100100010'B Assignment:[25] tcv_AuthAUTN_2 := (view Assignment) Assignment:[26] tcv_AuthAUTN := (view Assignment) Attach:[2] Exit Test Step ts_MM_AuthenticationInit::lt_AuthCalcAUTN
Attach:[3] Enter Test Step ts_MM_AuthenticationInit::lt_AuthCalcUMTS_Others( )
| Assignment:[27] tcv_AuthIK := (view Assignment) Assignment:[28] tcv_AuthCK := (view Assignment) Assignment:[29] tcv_AuthXRES := (view Assignment) Attach:[3] Exit Test Step ts_MM_AuthenticationInit::lt_AuthCalcUMTS_Others
Attach:[4] Enter Test Step ts_MM_AuthenticationInit::lt_AuthCalcKcGSM( )
| Assignment:[30] tcv_AuthCK_1 := '0100010001110111011001100001000100000000001100110010001011011101'B Assignment:[31] tcv_AuthCK_2 := '1100110011111111111011101001100110001000101110111010101001010101'B Assignment:[32] tcv_AuthIK_1 := '0111011101100110000100010000000000110011001000101101110111001100'B Assignment:[33] tcv_AuthIK_2 := '1111111111101110100110011000100010111011101010100101010101000100'B Assignment:[34] tcv_AuthCK_XOR := '1000100010001000100010001000100010001000100010001000100010001000'B Assignment:[35] tcv_AuthIK_XOR := '1000100010001000100010001000100010001000100010001000100010001000'B Assignment:[36] tcv_AuthKcGSM := '0000000000000000000000000000000000000000000000000000000000000000'B Attach:[4] Exit Test Step ts_MM_AuthenticationInit::lt_AuthCalcKcGSM
Attach:[1] Exit Test Step ts_MM_AuthenticationInit
00:03:27.620 - Primitive: RRC_DATA_REQ: mm:authenticationRequest 00:03:27.620 - Primitive: RLC_AM_DATA_REQ:downlinkDirectTransfer Send event:[2] Dc ! RRC_DataReq = PDU (view PDU) 00:03:27.610 - Primitive: RLC_AM_DATA_IND: initialDirectTransfer 00:03:27.610 - Primitive: RRC_DATA_IND: gmm:attachRequest begin "car_UplinkDirectTransfer" of type RRC_DataInd (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "rB_Id" of type SS_RB_Identity (INTEGER) [UNIVERSAL 2] matching 3 against 3 end "rB_Id" of type SS_RB_Identity begin "cN_Domain" of type SS_CN_DomainIdentity (INTEGER) [UNIVERSAL 2] matching 1 against 0 end "cN_Domain" of type SS_CN_DomainIdentity end "car_UplinkDirectTransfer" of type RRC_DataInd Match failed [#4] : (view details)
Expected | RRC_DataInd
Received | RRC_DataInd
begin "car_UplinkDirectTransfer" of type RRC_DataInd (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "rB_Id" of type SS_RB_Identity (INTEGER) [UNIVERSAL 2] matching 3 against 3 end "rB_Id" of type SS_RB_Identity begin "cN_Domain" of type SS_CN_DomainIdentity (INTEGER) [UNIVERSAL 2] matching 1 against 0 end "cN_Domain" of type SS_CN_DomainIdentity end "car_UplinkDirectTransfer" of type RRC_DataInd Match failed [#5] : (view details)
Expected | RRC_DataInd
Received | RRC_DataInd
begin "car_UplinkDirectTransfer" of type RRC_DataInd (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "rB_Id" of type SS_RB_Identity (INTEGER) [UNIVERSAL 2] matching 3 against 3 end "rB_Id" of type SS_RB_Identity begin "cN_Domain" of type SS_CN_DomainIdentity (INTEGER) [UNIVERSAL 2] matching 1 against 0 end "cN_Domain" of type SS_CN_DomainIdentity end "car_UplinkDirectTransfer" of type RRC_DataInd Match failed [#6] : (view details)
Expected | RRC_DataInd
Received | RRC_DataInd
begin "car_PS_InitDirectTransfer" of type RRC_DataInd (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "rB_Id" of type SS_RB_Identity (INTEGER) [UNIVERSAL 2] matching 3 against 3 end "rB_Id" of type SS_RB_Identity begin "cN_Domain" of type SS_CN_DomainIdentity (INTEGER) [UNIVERSAL 2] matching 1 against 1 end "cN_Domain" of type SS_CN_DomainIdentity begin "start" of type START_Value (BITSTRING) [UNIVERSAL 3] matching '00000000000000000010'B against ? end "start" of type START_Value begin "msg" of type ATTACHREQUEST (SEQUENCE) [UNIVERSAL 16] begin "skipIndicator" of type SkipIndicator (BITSTRING) [UNIVERSAL 3] matching '0000'B against '0000'B end "skipIndicator" of type SkipIndicator begin "gMMProtocolDiscriminator" of type ProtocolDiscriminator (BITSTRING) [UNIVERSAL 3] matching '1000'B against '1000'B end "gMMProtocolDiscriminator" of type ProtocolDiscriminator begin "msgType" of type MsgType (BITSTRING) [UNIVERSAL 3] matching '00000001'B against '00000001'B end "msgType" of type MsgType begin "msNetworkCap" of type MS_NetworkCap_lv (SEQUENCE) [UNIVERSAL 16] matching { iel: '02'O , value: 'E540'O } against ? end "msNetworkCap" of type MS_NetworkCap_lv begin "gprsCiphKeySeqNo" of type CiphKeySeqNum (SEQUENCE) [UNIVERSAL 16] begin "spare1" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against '0'B end "spare1" of type B1 begin "keySeq" of type KeySeq (BITSTRING) [UNIVERSAL 3] matching '111'B against ? end "keySeq" of type KeySeq end "gprsCiphKeySeqNo" of type CiphKeySeqNum begin "attachType" of type AttachType (SEQUENCE) [UNIVERSAL 16] begin "for" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against ? end "for" of type B1 begin "type" of type B3 (BITSTRING) [UNIVERSAL 3] matching '001'B against ? end "type" of type B3 end "attachType" of type AttachType begin "drxParameter" of type DRXparamter (SEQUENCE) [UNIVERSAL 16] matching { splitPGcycleCode: '00000111'B , cnDRXcoef: '0000'B , splitOnCCCH: '0'B , nonDRXtimer: '100'B } against ? end "drxParameter" of type DRXparamter begin "ptmsiORimsi" of type MS_Identity_lv (SEQUENCE) [UNIVERSAL 16] begin "iel" of type Length (OCTETSTRING) [UNIVERSAL 4] matching '08'O against ? end "iel" of type Length begin "iDigit1" of type B4 (BITSTRING) [UNIVERSAL 3] matching '0000'B against ? end "iDigit1" of type B4 begin "oddEvenInd" of type B1 (BITSTRING) [UNIVERSAL 3] matching '1'B against ? end "oddEvenInd" of type B1 begin "typeOfId" of type B3 (BITSTRING) [UNIVERSAL 3] matching '001'B against ? end "typeOfId" of type B3 begin "otherDigits" of type OCTETSTRING [UNIVERSAL 4] matching '10100000003033'O against ? end "otherDigits" of type OCTETSTRING end "ptmsiORimsi" of type MS_Identity_lv begin "oldRAI" of type RAI_v (SEQUENCE) [UNIVERSAL 16] begin "plmn" of type OCTETSTRING [UNIVERSAL 4] matching '00F110'O against ? end "plmn" of type OCTETSTRING begin "lac" of type OCTETSTRING [UNIVERSAL 4] matching 'FFFE'O against ? end "lac" of type OCTETSTRING begin "rac" of type OCTETSTRING [UNIVERSAL 4] matching '05'O against ? end "rac" of type OCTETSTRING end "oldRAI" of type RAI_v begin "msRadioAccessCap" of type MSRadioAccessCap_lv (SEQUENCE) [UNIVERSAL 16] matching { iel: '0B'O , value: '15F38233542A332644A198'O } against ? end "msRadioAccessCap" of type MSRadioAccessCap_lv begin "readyTimer" of type GPRS_Timer (SEQUENCE) [UNIVERSAL 16] begin "iei" of type IEI8 (BITSTRING) [UNIVERSAL 3] matching '00010111'B against '00010111'B end "iei" of type IEI8 begin "unit" of type B3 (BITSTRING) [UNIVERSAL 3] matching '000'B against ? end "unit" of type B3 begin "value" of type B5 (BITSTRING) [UNIVERSAL 3] matching '10110'B against ? end "value" of type B5 end "readyTimer" of type GPRS_Timer end "msg" of type ATTACHREQUEST end "car_PS_InitDirectTransfer" of type RRC_DataInd begin "car_PS_InitDirectTransfer" of type RRC_DataInd (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "rB_Id" of type SS_RB_Identity (INTEGER) [UNIVERSAL 2] matching 3 against 3 end "rB_Id" of type SS_RB_Identity begin "cN_Domain" of type SS_CN_DomainIdentity (INTEGER) [UNIVERSAL 2] matching 1 against 1 end "cN_Domain" of type SS_CN_DomainIdentity begin "start" of type START_Value (BITSTRING) [UNIVERSAL 3] matching '00000000000000000010'B against ? end "start" of type START_Value begin "msg" of type ATTACHREQUEST (SEQUENCE) [UNIVERSAL 16] begin "skipIndicator" of type SkipIndicator (BITSTRING) [UNIVERSAL 3] matching '0000'B against '0000'B end "skipIndicator" of type SkipIndicator begin "gMMProtocolDiscriminator" of type ProtocolDiscriminator (BITSTRING) [UNIVERSAL 3] matching '1000'B against '1000'B end "gMMProtocolDiscriminator" of type ProtocolDiscriminator begin "msgType" of type MsgType (BITSTRING) [UNIVERSAL 3] matching '00000001'B against '00000001'B end "msgType" of type MsgType begin "msNetworkCap" of type MS_NetworkCap_lv (SEQUENCE) [UNIVERSAL 16] matching { iel: '02'O , value: 'E540'O } against ? end "msNetworkCap" of type MS_NetworkCap_lv begin "gprsCiphKeySeqNo" of type CiphKeySeqNum (SEQUENCE) [UNIVERSAL 16] begin "spare1" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against '0'B end "spare1" of type B1 begin "keySeq" of type KeySeq (BITSTRING) [UNIVERSAL 3] matching '111'B against ? end "keySeq" of type KeySeq end "gprsCiphKeySeqNo" of type CiphKeySeqNum begin "attachType" of type AttachType (SEQUENCE) [UNIVERSAL 16] begin "for" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against ? end "for" of type B1 begin "type" of type B3 (BITSTRING) [UNIVERSAL 3] matching '001'B against ? end "type" of type B3 end "attachType" of type AttachType begin "drxParameter" of type DRXparamter (SEQUENCE) [UNIVERSAL 16] matching { splitPGcycleCode: '00000111'B , cnDRXcoef: '0000'B , splitOnCCCH: '0'B , nonDRXtimer: '100'B } against ? end "drxParameter" of type DRXparamter begin "ptmsiORimsi" of type MS_Identity_lv (SEQUENCE) [UNIVERSAL 16] begin "iel" of type Length (OCTETSTRING) [UNIVERSAL 4] matching '08'O against ? end "iel" of type Length begin "iDigit1" of type B4 (BITSTRING) [UNIVERSAL 3] matching '0000'B against ? end "iDigit1" of type B4 begin "oddEvenInd" of type B1 (BITSTRING) [UNIVERSAL 3] matching '1'B against ? end "oddEvenInd" of type B1 begin "typeOfId" of type B3 (BITSTRING) [UNIVERSAL 3] matching '001'B against ? end "typeOfId" of type B3 begin "otherDigits" of type OCTETSTRING [UNIVERSAL 4] matching '10100000003033'O against ? end "otherDigits" of type OCTETSTRING end "ptmsiORimsi" of type MS_Identity_lv begin "oldRAI" of type RAI_v (SEQUENCE) [UNIVERSAL 16] begin "plmn" of type OCTETSTRING [UNIVERSAL 4] matching '00F110'O against ? end "plmn" of type OCTETSTRING begin "lac" of type OCTETSTRING [UNIVERSAL 4] matching 'FFFE'O against ? end "lac" of type OCTETSTRING begin "rac" of type OCTETSTRING [UNIVERSAL 4] matching '05'O against ? end "rac" of type OCTETSTRING end "oldRAI" of type RAI_v begin "msRadioAccessCap" of type MSRadioAccessCap_lv (SEQUENCE) [UNIVERSAL 16] matching { iel: '0B'O , value: '15F38233542A332644A198'O } against ? end "msRadioAccessCap" of type MSRadioAccessCap_lv begin "readyTimer" of type GPRS_Timer (SEQUENCE) [UNIVERSAL 16] begin "iei" of type IEI8 (BITSTRING) [UNIVERSAL 3] matching '00010111'B against '00010111'B end "iei" of type IEI8 begin "unit" of type B3 (BITSTRING) [UNIVERSAL 3] matching '000'B against ? end "unit" of type B3 begin "value" of type B5 (BITSTRING) [UNIVERSAL 3] matching '10110'B against ? end "value" of type B5 end "readyTimer" of type GPRS_Timer end "msg" of type ATTACHREQUEST end "car_PS_InitDirectTransfer" of type RRC_DataInd Assignment:[19] tcv_TmpAttachReqPDU (view PDU) Assignment:[19] tcv_TmpB3 := '001'B Assignment:[19] start_PS := '00000000000000000010'B Assignment:[19] tcv_GMM_AttachRec := GcTRUE Receive event:[19] Dc ? RRC_DataInd = PDU (view PDU) 00:03:28.060 - Primitive: RLC_AM_DATA_IND: uplinkDirectTransfer 00:03:28.060 - Primitive: RRC_DATA_IND: mm:authenticationResponse begin "car_UplinkDirectTransfer" of type RRC_DataInd (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "rB_Id" of type SS_RB_Identity (INTEGER) [UNIVERSAL 2] matching 3 against 3 end "rB_Id" of type SS_RB_Identity begin "cN_Domain" of type SS_CN_DomainIdentity (INTEGER) [UNIVERSAL 2] matching 0 against 0 end "cN_Domain" of type SS_CN_DomainIdentity begin "msg" of type AUTHENTICATIONRESPONSE (SEQUENCE) [UNIVERSAL 16] begin "skipIndicator" of type SkipIndicator (BITSTRING) [UNIVERSAL 3] matching '0000'B against '0000'B end "skipIndicator" of type SkipIndicator begin "mMProtocolDiscriminator" of type ProtocolDiscriminator (BITSTRING) [UNIVERSAL 3] matching '0101'B against '0101'B end "mMProtocolDiscriminator" of type ProtocolDiscriminator begin "msgType" of type MsgType (BITSTRING) [UNIVERSAL 3] matching '01010100'B against '??010100'B end "msgType" of type MsgType begin "authRsp" of type AuthRsp (BITSTRING) [UNIVERSAL 3] matching '01010101010001000111011101100110'B against ? end "authRsp" of type AuthRsp begin "authRspExt" of type AuthRspExt (SEQUENCE) [UNIVERSAL 16] begin "iei" of type IEI8 (BITSTRING) [UNIVERSAL 3] matching '00100001'B against '00100001'B end "iei" of type IEI8 begin "iel" of type Length (OCTETSTRING) [UNIVERSAL 4] matching '04'O against ? end "iel" of type Length begin "rES" of type BITSTRING [UNIVERSAL 3] matching '00010001000000000011001100100010'B against ? end "rES" of type BITSTRING end "authRspExt" of type AuthRspExt end "msg" of type AUTHENTICATIONRESPONSE end "car_UplinkDirectTransfer" of type RRC_DataInd Assignment:[3] tcv_AuthRspPDU (view PDU) Assignment:[3] tcv_AuthRsp := '01010101010001000111011101100110'B Assignment:[3] tcv_AuthRspExt := { iei: '00100001'B , iel: '04'O , rES: '00010001000000000011001100100010'B } Receive event:[3] Dc ? RRC_DataInd = PDU (view PDU) Assignment:[4] tcv_Res := GcTRUE Attach:[4] Exit Test Step ts_MM_Authentication
Attach:[5] Enter Test Step ts_RRC_Security( 3 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 3 )
| Assignment:[8] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[2] Enter Test Step ts_RRC_Security::lt_RRC_InitVariables( 3 )
| Attach:[53] Enter Test Step ts_RRC_Security::lt_InitCipherMode( 3 )
| Assignment:[82] cs_cipheringStarted := GcFALSE Assignment:[82] ps_cipheringStarted := GcFALSE Assignment:[84] cipheringAlgorithmCapability := '0000000000000011'B Attach:[53] Exit Test Step ts_RRC_Security::lt_InitCipherMode
Attach:[54] Enter Test Step ts_RRC_Security::lt_InitIntegrity( 3 )
| Assignment:[87] recentSecureDomain := cs_domain Assignment:[92] dL_Integrity := (view Assignment) Assignment:[92] integrityStarted := GcTRUE Assignment:[92] dl_IntegrityCheckInfo := (view Assignment) Assignment:[92] tcv_Int_ModifyFlag := GcFALSE Attach:[54] Exit Test Step ts_RRC_Security::lt_InitIntegrity
Attach:[55] Enter Test Step ts_InitSystemSpecificCap( )
| Assignment:[11] tcv_UE_SystemSpecificCap := 0 Attach:[55] Exit Test Step ts_InitSystemSpecificCap
Attach:[56] Enter Test Step ts_SaveCellInfo( 3 )
| Assignment:[8] tcv_CellInfoD := (view Assignment) Attach:[56] Exit Test Step ts_SaveCellInfo
Assignment:[58] tcv_HFN := '00000000000000000000'B Assignment:[60] start_CS := '00000000000000000000'B Attach:[2] Exit Test Step ts_RRC_Security::lt_RRC_InitVariables
Attach:[3] Enter Test Step ts_SS_DownloadSecurityKey( 3 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 3 )
| Assignment:[8] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[15] Enter Test Step ts_SS_DownloadSecurityKey::lt_DownloadKeyCRLC( '00000000000000000000'B )
| 00:03:28.070 - Primitive: CRLC_SecurityMode_Config_REQ 00:03:28.070 - Primitive: CRLC_SecurityMode_Config_REQ Send event:[21] CRLC ! CRLC_SecurityMode_Config_REQ = PDU (view PDU) 00:03:28.090 - Primitive: CRLC_SecurityMode_Config_CNF begin "ca_CRLC_SecurityModeCfgCnf" of type CRLC_SecurityMode_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER end "ca_CRLC_SecurityModeCfgCnf" of type CRLC_SecurityMode_Config_CNF Receive event:[22] CRLC ? CRLC_SecurityMode_Config_CNF = PDU: { cellId: -1 } Attach:[15] Exit Test Step ts_SS_DownloadSecurityKey::lt_DownloadKeyCRLC
Attach:[3] Exit Test Step ts_SS_DownloadSecurityKey
Attach:[4] Enter Test Step ts_RRC_Security::lt_ActivateSecurity_DL_SS( 3 )
| Attach:[14] Enter Test Step ts_RRC_Security::lt_InitialiseRRC_MSN( 3 )
| Attach:[25] Enter Test Step ts_SetDL_RRC_MessageSN( 3 )
| 00:03:28.090 - Primitive: CRLC_SetRRC_MessageSN_REQ Send event:[1] CRLC ! CRLC_SetRRC_MessageSN_REQ = PDU (view PDU) 00:03:28.100 - Primitive: CRLC_SetRRC_MessageSN_CNF begin "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF Receive event:[2] CRLC ? CRLC_SetRRC_MessageSN_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: 0 ]} 00:03:28.100 - Primitive: CRLC_SetRRC_MessageSN_REQ Send event:[3] CRLC ! CRLC_SetRRC_MessageSN_REQ = PDU (view PDU) 00:03:28.120 - Primitive: CRLC_SetRRC_MessageSN_CNF begin "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF Receive event:[4] CRLC ? CRLC_SetRRC_MessageSN_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 1 ]} 00:03:28.120 - Primitive: CRLC_SetRRC_MessageSN_REQ Send event:[5] CRLC ! CRLC_SetRRC_MessageSN_REQ = PDU (view PDU) 00:03:28.130 - Primitive: CRLC_SetRRC_MessageSN_CNF begin "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF Receive event:[6] CRLC ? CRLC_SetRRC_MessageSN_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 2 ]} 00:03:28.130 - Primitive: CRLC_SetRRC_MessageSN_REQ Send event:[7] CRLC ! CRLC_SetRRC_MessageSN_REQ = PDU (view PDU) 00:03:28.150 - Primitive: CRLC_SetRRC_MessageSN_CNF begin "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF Receive event:[8] CRLC ? CRLC_SetRRC_MessageSN_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 3 ]} 00:03:28.150 - Primitive: CRLC_SetRRC_MessageSN_REQ Send event:[9] CRLC ! CRLC_SetRRC_MessageSN_REQ = PDU (view PDU) 00:03:28.170 - Primitive: CRLC_SetRRC_MessageSN_CNF begin "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF Receive event:[10] CRLC ? CRLC_SetRRC_MessageSN_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 4 ]} Attach:[25] Exit Test Step ts_SetDL_RRC_MessageSN
Attach:[14] Exit Test Step ts_RRC_Security::lt_InitialiseRRC_MSN
Attach:[15] Enter Test Step ts_CRLC_DL_Integrity( { integrityProtectionM ...
| (view Test Step parameters) 00:03:28.170 - Primitive: CRLC_Integrity_Activate_REQ 00:03:28.170 - Primitive: CRLC_Integrity_Activate_REQ Send event:[1] CRLC ! CRLC_Integrity_Activate_REQ = PDU (view PDU) 00:03:28.180 - Primitive: CRLC_Integrity_Activate_CNF begin "ca_CRLC_IntegrityActivateCnf" of type CRLC_Integrity_Activate_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER end "ca_CRLC_IntegrityActivateCnf" of type CRLC_Integrity_Activate_CNF Receive event:[2] CRLC ? CRLC_Integrity_Activate_CNF = PDU: { cellId: -1 } Attach:[15] Exit Test Step ts_CRLC_DL_Integrity
Attach:[4] Exit Test Step ts_RRC_Security::lt_ActivateSecurity_DL_SS
Attach:[5] Enter Test Step ts_RRC_Security::lt_RB2_UL_IntegrityActivate( 3 )
| Attach:[13] Enter Test Step ts_RB2_UL_IntegrityActivate( 0 )
| 00:03:28.180 - Primitive: CRLC_Integrity_Activate_REQ 00:03:28.180 - Primitive: CRLC_Integrity_Activate_REQ Send event:[1] CRLC ! CRLC_Integrity_Activate_REQ = PDU (view PDU) 00:03:28.200 - Primitive: CRLC_Integrity_Activate_CNF begin "ca_CRLC_IntegrityActivateCnf" of type CRLC_Integrity_Activate_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER end "ca_CRLC_IntegrityActivateCnf" of type CRLC_Integrity_Activate_CNF Receive event:[2] CRLC ? CRLC_Integrity_Activate_CNF = PDU: { cellId: -1 } Attach:[13] Exit Test Step ts_RB2_UL_IntegrityActivate
Attach:[5] Exit Test Step ts_RRC_Security::lt_RB2_UL_IntegrityActivate
Attach:[6] Enter Test Step ts_RRC_Security::lt_StartSecurity_UE( 3 )
| Attach:[27] Enter Test Step ts_RRC_Security::lt_SendSecurityModeCommand( 3 )
| 00:03:28.200 - Primitive: RLC_AM_DATA_REQ 00:03:28.200 - Primitive: RLC_AM_DATA_REQ: securityModeCommand Send event:[52] AM ! RLC_AM_DATA_REQ = PDU (view PDU) Attach:[27] Exit Test Step ts_RRC_Security::lt_SendSecurityModeCommand
00:03:28.460 - Primitive: RLC_AM_DATA_IND: securityModeComplete 00:03:28.460 - Primitive: RLC_AM_DATA_IND begin "car_RRC_SecModeCmpl" of type RLC_AM_DATA_IND (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "integrityResult" of type IntegrityResult (CHOICE) [UNIVERSAL 31] matching [integrityUsed: i_pass] against * end "integrityResult" of type IntegrityResult begin "aM_message" of type CHOICE [UNIVERSAL 31] begin "uL_DCCH_Message" of type UL_DCCH_Message (SEQUENCE) [UNIVERSAL 16] begin "integrityCheckInfo" of type IntegrityCheckInfo (SEQUENCE) [UNIVERSAL 16] matching { messageAuthenticationCode: '10001011001000110111110011100010'B , rrc_MessageSequenceNumber: 1 } against * end "integrityCheckInfo" of type IntegrityCheckInfo begin "message" of type UL_DCCH_MessageType (CHOICE) [UNIVERSAL 31] begin "securityModeComplete" of type SecurityModeComplete (SEQUENCE) [UNIVERSAL 16] begin "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier (INTEGER) [UNIVERSAL 2] matching 0 against 0 end "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier begin "ul_IntegProtActivationInfo" of type IntegrityProtActivationInfo (SEQUENCE) [UNIVERSAL 16] matching { rrc_MessageSequenceNumberList: [ 0 , 0 , 0 , 0 , 0 ] } against * end "ul_IntegProtActivationInfo" of type IntegrityProtActivationInfo end "securityModeComplete" of type SecurityModeComplete end "message" of type UL_DCCH_MessageType end "uL_DCCH_Message" of type UL_DCCH_Message end "aM_message" of type CHOICE end "car_RRC_SecModeCmpl" of type RLC_AM_DATA_IND Assignment:TSP2: [34] uL_Integrity := { rrc_MessageSequenceNumberList: [ 0 , 0 , 0 , 0 , 0 ] } Receive event:TSP2: [34] AM ? RLC_AM_DATA_IND = PDU (view PDU) Preliminary verdict:TSP2: [34] (PASS) Attach:[35] Enter Test Step ts_CRLC_UL_Integrity( { rrc_MessageSequenceNumberList: [ 0 , 0 , 0 , 0 , 0 ] } )
| 00:03:28.460 - Primitive: CRLC_Integrity_Activate_REQ 00:03:28.460 - Primitive: CRLC_Integrity_Activate_REQ Send event:[1] CRLC ! CRLC_Integrity_Activate_REQ = PDU (view PDU) 00:03:28.480 - Primitive: CRLC_Integrity_Activate_CNF begin "ca_CRLC_IntegrityActivateCnf" of type CRLC_Integrity_Activate_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER end "ca_CRLC_IntegrityActivateCnf" of type CRLC_Integrity_Activate_CNF Receive event:[2] CRLC ? CRLC_Integrity_Activate_CNF = PDU: { cellId: -1 } Attach:[35] Exit Test Step ts_CRLC_UL_Integrity
Attach:[6] Exit Test Step ts_RRC_Security::lt_StartSecurity_UE
Attach:[5] Exit Test Step ts_RRC_Security
Assignment:[6] tcv_AssignedTMSI := '11223344'O 00:03:28.480 - Primitive: RRC_DATA_REQ: mm:locationUpdatingAccept 00:03:28.480 - Primitive: RLC_AM_DATA_REQ:downlinkDirectTransfer Send event:[6] Dc ! RRC_DataReq = PDU (view PDU) 00:03:28.760 - Primitive: RLC_AM_DATA_IND: uplinkDirectTransfer 00:03:28.760 - Primitive: RRC_DATA_IND: mm:tmsiReallocationComplete begin "car_UplinkDirectTransfer" of type RRC_DataInd (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "rB_Id" of type SS_RB_Identity (INTEGER) [UNIVERSAL 2] matching 3 against 3 end "rB_Id" of type SS_RB_Identity begin "cN_Domain" of type SS_CN_DomainIdentity (INTEGER) [UNIVERSAL 2] matching 0 against 0 end "cN_Domain" of type SS_CN_DomainIdentity begin "msg" of type TMSIREALLOCATIONCOMPLETE (SEQUENCE) [UNIVERSAL 16] begin "skipIndicator" of type SkipIndicator (BITSTRING) [UNIVERSAL 3] matching '0000'B against '0000'B end "skipIndicator" of type SkipIndicator begin "mMProtocolDiscriminator" of type ProtocolDiscriminator (BITSTRING) [UNIVERSAL 3] matching '0101'B against '0101'B end "mMProtocolDiscriminator" of type ProtocolDiscriminator begin "msgType" of type MsgType (BITSTRING) [UNIVERSAL 3] matching '10011011'B against '??011011'B end "msgType" of type MsgType end "msg" of type TMSIREALLOCATIONCOMPLETE end "car_UplinkDirectTransfer" of type RRC_DataInd Receive event:[7] Dc ? RRC_DataInd = PDU (view PDU) Attach:[4] Exit Test Step ts_RegistrationOnCS
Attach:[5] Enter Test Step ts_MM_RegistrationHandleAttachReqIMSI::lt_HandleAttachReqA( 3 )
| Assignment:[8] tcv_GMM_AttachExpect := GcFALSE Assignment:[10] tcv_Start := '00000000000000000010'B Preliminary verdict:TSP1: [11] (PASS) Attach:[5] Exit Test Step ts_MM_RegistrationHandleAttachReqIMSI::lt_HandleAttachReqA
Attach:[38] Exit Test Step ts_MM_RegistrationHandleAttachReqIMSI
Attach:[39] Enter Test Step ts_GMM_AuthenticateAndStartIntegrityProtection( 3 )
| Attach:[1] Enter Test Step ts_GMM_Authentication( 3 )
| Attach:[1] Enter Test Step ts_GMM_AuthenticationInit( )
| Attach:[1] Enter Test Step ts_GMM_AuthenticationInit::lt_IncrementCiphKeySeqNum( )
| Assignment:[18] tcv_PS_KeySeq := '000'B Attach:[1] Exit Test Step ts_GMM_AuthenticationInit::lt_IncrementCiphKeySeqNum
Attach:[2] Enter Test Step ts_GMM_AuthenticationInit::lt_AuthCalcAUTN( )
| Assignment:[19] tcv_AuthXDOUT := (view Assignment) Assignment:[20] tcv_AuthCDOUT := '0000000000000000000000000000000000000000000000000000000000000000'B Assignment:[21] tcv_AuthXDOUT_Half := '0101010101000100011101110110011000010001000000000011001100100010'B Assignment:[22] tcv_AuthAK := '011001100001000100000000001100110010001011011101'B Assignment:[23] tcv_AuthAUTN_1 := '011001100001000100000000001100110010001011011101'B Assignment:[24] tcv_AuthMAC := '0101010101000100011101110110011000010001000000000011001100100010'B Assignment:[25] tcv_AuthAUTN_2 := (view Assignment) Assignment:[26] tcv_AuthAUTN := (view Assignment) Attach:[2] Exit Test Step ts_GMM_AuthenticationInit::lt_AuthCalcAUTN
Attach:[3] Enter Test Step ts_GMM_AuthenticationInit::lt_AuthCalcUMTS_Others( )
| Assignment:[27] tcv_PS_AuthIK := (view Assignment) Assignment:[28] tcv_PS_AuthCK := (view Assignment) Assignment:[29] tcv_AuthXRES := (view Assignment) Attach:[3] Exit Test Step ts_GMM_AuthenticationInit::lt_AuthCalcUMTS_Others
Attach:[4] Enter Test Step ts_GMM_AuthenticationInit::lt_AuthCalcKcGSM( )
| Assignment:[30] tcv_AuthCK_1 := '0100010001110111011001100001000100000000001100110010001011011101'B Assignment:[31] tcv_AuthCK_2 := '1100110011111111111011101001100110001000101110111010101001010101'B Assignment:[32] tcv_AuthIK_1 := '0111011101100110000100010000000000110011001000101101110111001100'B Assignment:[33] tcv_AuthIK_2 := '1111111111101110100110011000100010111011101010100101010101000100'B Assignment:[34] tcv_AuthCK_XOR := '1000100010001000100010001000100010001000100010001000100010001000'B Assignment:[35] tcv_AuthIK_XOR := '1000100010001000100010001000100010001000100010001000100010001000'B Assignment:[36] tcv_AuthKcGSM := '0000000000000000000000000000000000000000000000000000000000000000'B Attach:[4] Exit Test Step ts_GMM_AuthenticationInit::lt_AuthCalcKcGSM
Attach:[1] Exit Test Step ts_GMM_AuthenticationInit
00:03:28.780 - Primitive: RRC_DATA_REQ: gmm:authenticationAndCipheringRequest 00:03:28.780 - Primitive: RLC_AM_DATA_REQ:downlinkDirectTransfer Send event:[2] Dc ! RRC_DataReq = PDU (view PDU) 00:03:29.240 - Primitive: RLC_AM_DATA_IND: uplinkDirectTransfer 00:03:29.240 - Primitive: RRC_DATA_IND: gmm:authenticationAndCipheringResponse begin "car_PS_UplinkDirectTransfer" of type RRC_DataInd (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "rB_Id" of type SS_RB_Identity (INTEGER) [UNIVERSAL 2] matching 3 against 3 end "rB_Id" of type SS_RB_Identity begin "cN_Domain" of type SS_CN_DomainIdentity (INTEGER) [UNIVERSAL 2] matching 1 against 1 end "cN_Domain" of type SS_CN_DomainIdentity begin "msg" of type AUTHENTICATIONANDCIPHERINGRESPONSE (SEQUENCE) [UNIVERSAL 16] begin "skipIndicator" of type SkipIndicator (BITSTRING) [UNIVERSAL 3] matching '0000'B against '0000'B end "skipIndicator" of type SkipIndicator begin "gMMProtocolDiscriminator" of type ProtocolDiscriminator (BITSTRING) [UNIVERSAL 3] matching '1000'B against '1000'B end "gMMProtocolDiscriminator" of type ProtocolDiscriminator begin "msgType" of type MsgType (BITSTRING) [UNIVERSAL 3] matching '00010011'B against '00010011'B end "msgType" of type MsgType begin "spare4" of type B4 (BITSTRING) [UNIVERSAL 3] matching '0000'B against '0000'B end "spare4" of type B4 begin "acRefNo" of type AC_ReferenceNumber (SEQUENCE) [UNIVERSAL 16] matching { value: '0011'B } against ? end "acRefNo" of type AC_ReferenceNumber begin "authRsp" of type AuthRsp_tv (SEQUENCE) [UNIVERSAL 16] begin "iei" of type IEI8 (BITSTRING) [UNIVERSAL 3] matching '00100010'B against '00100010'B end "iei" of type IEI8 begin "value" of type BITSTRING [UNIVERSAL 3] matching '01010101010001000111011101100110'B against ? end "value" of type BITSTRING end "authRsp" of type AuthRsp_tv begin "authRspExt" of type AuthRspExt (SEQUENCE) [UNIVERSAL 16] begin "iei" of type IEI8 (BITSTRING) [UNIVERSAL 3] matching '00101001'B against '00101001'B end "iei" of type IEI8 begin "iel" of type Length (OCTETSTRING) [UNIVERSAL 4] matching '04'O against ? end "iel" of type Length begin "rES" of type BITSTRING [UNIVERSAL 3] matching '00010001000000000011001100100010'B against ? end "rES" of type BITSTRING end "authRspExt" of type AuthRspExt end "msg" of type AUTHENTICATIONANDCIPHERINGRESPONSE end "car_PS_UplinkDirectTransfer" of type RRC_DataInd Assignment:[3] tcv_TmpAuthAndCiphRspPDU (view PDU) Assignment:[3] tcv_AuthRsp := '01010101010001000111011101100110'B Assignment:[3] tcv_AuthRspExt := { iei: '00101001'B , iel: '04'O , rES: '00010001000000000011001100100010'B } Receive event:[3] Dc ? RRC_DataInd = PDU (view PDU) Assignment:[4] tcv_Res := GcTRUE Preliminary verdict:TSP1: [6] (PASS) Attach:[1] Exit Test Step ts_GMM_Authentication
Attach:[2] Enter Test Step ts_RRC_Security( 3 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 3 )
| Assignment:[8] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[2] Enter Test Step ts_RRC_Security::lt_RRC_InitVariables( 3 )
| Attach:[53] Enter Test Step ts_RRC_Security::lt_InitCipherMode( 3 )
| Assignment:[82] cs_cipheringStarted := GcFALSE Assignment:[82] ps_cipheringStarted := GcFALSE Assignment:[84] cipheringAlgorithmCapability := '0000000000000011'B Attach:[53] Exit Test Step ts_RRC_Security::lt_InitCipherMode
Attach:[54] Enter Test Step ts_RRC_Security::lt_InitIntegrity( 3 )
| Assignment:[87] recentSecureDomain := ps_domain Attach:[89] Enter Test Step ts_GetRRC_MessageSN( 3 )
| 00:03:29.240 - Primitive: CRLC_RRC_MessageSN_REQ Send event:[1] CRLC ! CRLC_RRC_MessageSN_REQ = PDU: { cellId: -1 , routingInfo: [rB_Identity: 0 ]} 00:03:29.260 - Primitive: CRLC_RRC_MessageSN_CNF begin "car_CRLC_RRC_MessageSN_CNF" of type CRLC_RRC_MessageSN_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "count_I_MSB_UL" of type COUNT_I_MSB (INTEGER) [UNIVERSAL 2] matching 0 against ? end "count_I_MSB_UL" of type COUNT_I_MSB begin "count_I_LSB_UL" of type RRC_SequenceNumber (INTEGER) [UNIVERSAL 2] matching 0 against ? end "count_I_LSB_UL" of type RRC_SequenceNumber begin "count_I_MSB_DL" of type COUNT_I_MSB (INTEGER) [UNIVERSAL 2] matching 0 against ? end "count_I_MSB_DL" of type COUNT_I_MSB begin "count_I_LSB_DL" of type RRC_SequenceNumber (INTEGER) [UNIVERSAL 2] matching 0 against ? end "count_I_LSB_DL" of type RRC_SequenceNumber end "car_CRLC_RRC_MessageSN_CNF" of type CRLC_RRC_MessageSN_CNF Assignment:[2] tcv_RRC_MSN_RB0 := 0 Receive event:[2] CRLC ? CRLC_RRC_MessageSN_CNF = PDU (view PDU) 00:03:29.260 - Primitive: CRLC_RRC_MessageSN_REQ Send event:[3] CRLC ! CRLC_RRC_MessageSN_REQ = PDU: { cellId: -1 , routingInfo: [rB_Identity: 1 ]} 00:03:29.280 - Primitive: CRLC_RRC_MessageSN_CNF begin "car_CRLC_RRC_MessageSN_CNF" of type CRLC_RRC_MessageSN_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "count_I_MSB_UL" of type COUNT_I_MSB (INTEGER) [UNIVERSAL 2] matching 0 against ? end "count_I_MSB_UL" of type COUNT_I_MSB begin "count_I_LSB_UL" of type RRC_SequenceNumber (INTEGER) [UNIVERSAL 2] matching 0 against ? end "count_I_LSB_UL" of type RRC_SequenceNumber begin "count_I_MSB_DL" of type COUNT_I_MSB (INTEGER) [UNIVERSAL 2] matching 0 against ? end "count_I_MSB_DL" of type COUNT_I_MSB begin "count_I_LSB_DL" of type RRC_SequenceNumber (INTEGER) [UNIVERSAL 2] matching 0 against ? end "count_I_LSB_DL" of type RRC_SequenceNumber end "car_CRLC_RRC_MessageSN_CNF" of type CRLC_RRC_MessageSN_CNF Assignment:[4] tcv_RRC_MSN_RB1 := 0 Receive event:[4] CRLC ? CRLC_RRC_MessageSN_CNF = PDU (view PDU) 00:03:29.280 - Primitive: CRLC_RRC_MessageSN_REQ Send event:[5] CRLC ! CRLC_RRC_MessageSN_REQ = PDU: { cellId: -1 , routingInfo: [rB_Identity: 2 ]} 00:03:29.290 - Primitive: CRLC_RRC_MessageSN_CNF begin "car_CRLC_RRC_MessageSN_CNF" of type CRLC_RRC_MessageSN_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "count_I_MSB_UL" of type COUNT_I_MSB (INTEGER) [UNIVERSAL 2] matching 0 against ? end "count_I_MSB_UL" of type COUNT_I_MSB begin "count_I_LSB_UL" of type RRC_SequenceNumber (INTEGER) [UNIVERSAL 2] matching 1 against ? end "count_I_LSB_UL" of type RRC_SequenceNumber begin "count_I_MSB_DL" of type COUNT_I_MSB (INTEGER) [UNIVERSAL 2] matching 0 against ? end "count_I_MSB_DL" of type COUNT_I_MSB begin "count_I_LSB_DL" of type RRC_SequenceNumber (INTEGER) [UNIVERSAL 2] matching 1 against ? end "count_I_LSB_DL" of type RRC_SequenceNumber end "car_CRLC_RRC_MessageSN_CNF" of type CRLC_RRC_MessageSN_CNF Assignment:[6] tcv_RRC_MSN_RB2 := 1 Assignment:[6] tcv_RRC_MSN_RB2_UL := 1 Receive event:[6] CRLC ? CRLC_RRC_MessageSN_CNF = PDU (view PDU) 00:03:29.290 - Primitive: CRLC_RRC_MessageSN_REQ Send event:[7] CRLC ! CRLC_RRC_MessageSN_REQ = PDU: { cellId: -1 , routingInfo: [rB_Identity: 3 ]} 00:03:29.310 - Primitive: CRLC_RRC_MessageSN_CNF begin "car_CRLC_RRC_MessageSN_CNF" of type CRLC_RRC_MessageSN_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "count_I_MSB_UL" of type COUNT_I_MSB (INTEGER) [UNIVERSAL 2] matching 0 against ? end "count_I_MSB_UL" of type COUNT_I_MSB begin "count_I_LSB_UL" of type RRC_SequenceNumber (INTEGER) [UNIVERSAL 2] matching 2 against ? end "count_I_LSB_UL" of type RRC_SequenceNumber begin "count_I_MSB_DL" of type COUNT_I_MSB (INTEGER) [UNIVERSAL 2] matching 0 against ? end "count_I_MSB_DL" of type COUNT_I_MSB begin "count_I_LSB_DL" of type RRC_SequenceNumber (INTEGER) [UNIVERSAL 2] matching 2 against ? end "count_I_LSB_DL" of type RRC_SequenceNumber end "car_CRLC_RRC_MessageSN_CNF" of type CRLC_RRC_MessageSN_CNF Assignment:[8] tcv_RRC_MSN_RB3 := 2 Receive event:[8] CRLC ? CRLC_RRC_MessageSN_CNF = PDU (view PDU) 00:03:29.310 - Primitive: CRLC_RRC_MessageSN_REQ Send event:[9] CRLC ! CRLC_RRC_MessageSN_REQ = PDU: { cellId: -1 , routingInfo: [rB_Identity: 4 ]} 00:03:29.320 - Primitive: CRLC_RRC_MessageSN_CNF begin "car_CRLC_RRC_MessageSN_CNF" of type CRLC_RRC_MessageSN_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "count_I_MSB_UL" of type COUNT_I_MSB (INTEGER) [UNIVERSAL 2] matching 0 against ? end "count_I_MSB_UL" of type COUNT_I_MSB begin "count_I_LSB_UL" of type RRC_SequenceNumber (INTEGER) [UNIVERSAL 2] matching 0 against ? end "count_I_LSB_UL" of type RRC_SequenceNumber begin "count_I_MSB_DL" of type COUNT_I_MSB (INTEGER) [UNIVERSAL 2] matching 0 against ? end "count_I_MSB_DL" of type COUNT_I_MSB begin "count_I_LSB_DL" of type RRC_SequenceNumber (INTEGER) [UNIVERSAL 2] matching 0 against ? end "count_I_LSB_DL" of type RRC_SequenceNumber end "car_CRLC_RRC_MessageSN_CNF" of type CRLC_RRC_MessageSN_CNF Assignment:[10] tcv_RRC_MSN_RB4 := 0 Receive event:[10] CRLC ? CRLC_RRC_MessageSN_CNF = PDU (view PDU) Attach:[89] Exit Test Step ts_GetRRC_MessageSN
Assignment:[90] dL_Integrity := (view Assignment) Assignment:[90] tcv_Int_ModifyFlag := GcTRUE Attach:[54] Exit Test Step ts_RRC_Security::lt_InitIntegrity
Attach:[55] Enter Test Step ts_InitSystemSpecificCap( )
| Assignment:[11] tcv_UE_SystemSpecificCap := 0 Attach:[55] Exit Test Step ts_InitSystemSpecificCap
Attach:[56] Enter Test Step ts_SaveCellInfo( 3 )
| Assignment:[8] tcv_CellInfoD := (view Assignment) Attach:[56] Exit Test Step ts_SaveCellInfo
Assignment:[58] tcv_HFN := '00000000000000000000'B Assignment:[62] start_PS := '00000000000000000000'B Attach:[2] Exit Test Step ts_RRC_Security::lt_RRC_InitVariables
Attach:[3] Enter Test Step ts_SS_DownloadSecurityKey( 3 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 3 )
| Assignment:[8] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[15] Enter Test Step ts_SS_DownloadSecurityKey::lt_DownloadKeyCRLC( '00000000000000000000'B )
| 00:03:29.320 - Primitive: CRLC_SecurityMode_Config_REQ 00:03:29.320 - Primitive: CRLC_SecurityMode_Config_REQ Send event:[21] CRLC ! CRLC_SecurityMode_Config_REQ = PDU (view PDU) 00:03:29.340 - Primitive: CRLC_SecurityMode_Config_CNF begin "ca_CRLC_SecurityModeCfgCnf" of type CRLC_SecurityMode_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER end "ca_CRLC_SecurityModeCfgCnf" of type CRLC_SecurityMode_Config_CNF Receive event:[22] CRLC ? CRLC_SecurityMode_Config_CNF = PDU: { cellId: -1 } Attach:[15] Exit Test Step ts_SS_DownloadSecurityKey::lt_DownloadKeyCRLC
Attach:[3] Exit Test Step ts_SS_DownloadSecurityKey
Attach:[4] Enter Test Step ts_RRC_Security::lt_ActivateSecurity_DL_SS( 3 )
| Attach:[14] Enter Test Step ts_RRC_Security::lt_InitialiseRRC_MSN( 3 )
| Attach:[14] Exit Test Step ts_RRC_Security::lt_InitialiseRRC_MSN
Attach:[15] Enter Test Step ts_CRLC_DL_Integrity( { integrityProtectionM ...
| (view Test Step parameters) 00:03:29.340 - Primitive: CRLC_Integrity_Activate_REQ 00:03:29.340 - Primitive: CRLC_Integrity_Activate_REQ Send event:[1] CRLC ! CRLC_Integrity_Activate_REQ = PDU (view PDU) 00:03:29.350 - Primitive: CRLC_Integrity_Activate_CNF begin "ca_CRLC_IntegrityActivateCnf" of type CRLC_Integrity_Activate_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER end "ca_CRLC_IntegrityActivateCnf" of type CRLC_Integrity_Activate_CNF Receive event:[2] CRLC ? CRLC_Integrity_Activate_CNF = PDU: { cellId: -1 } Attach:[15] Exit Test Step ts_CRLC_DL_Integrity
Attach:[4] Exit Test Step ts_RRC_Security::lt_ActivateSecurity_DL_SS
Attach:[5] Enter Test Step ts_RRC_Security::lt_RB2_UL_IntegrityActivate( 3 )
| Attach:[11] Enter Test Step ts_RB2_UL_IntegrityActivate( 1 )
| 00:03:29.350 - Primitive: CRLC_Integrity_Activate_REQ 00:03:29.350 - Primitive: CRLC_Integrity_Activate_REQ Send event:[1] CRLC ! CRLC_Integrity_Activate_REQ = PDU (view PDU) 00:03:29.370 - Primitive: CRLC_Integrity_Activate_CNF begin "ca_CRLC_IntegrityActivateCnf" of type CRLC_Integrity_Activate_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER end "ca_CRLC_IntegrityActivateCnf" of type CRLC_Integrity_Activate_CNF Receive event:[2] CRLC ? CRLC_Integrity_Activate_CNF = PDU: { cellId: -1 } Attach:[11] Exit Test Step ts_RB2_UL_IntegrityActivate
Attach:[5] Exit Test Step ts_RRC_Security::lt_RB2_UL_IntegrityActivate
Attach:[6] Enter Test Step ts_RRC_Security::lt_StartSecurity_UE( 3 )
| Attach:[27] Enter Test Step ts_RRC_Security::lt_SendSecurityModeCommand( 3 )
| 00:03:29.370 - Primitive: RLC_AM_DATA_REQ 00:03:29.370 - Primitive: RLC_AM_DATA_REQ: securityModeCommand Send event:[52] AM ! RLC_AM_DATA_REQ = PDU (view PDU) Attach:[27] Exit Test Step ts_RRC_Security::lt_SendSecurityModeCommand
00:03:29.630 - Primitive: RLC_AM_DATA_IND: securityModeComplete 00:03:29.630 - Primitive: RLC_AM_DATA_IND begin "car_RRC_SecModeCmpl" of type RLC_AM_DATA_IND (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "integrityResult" of type IntegrityResult (CHOICE) [UNIVERSAL 31] matching [integrityUsed: i_pass] against * end "integrityResult" of type IntegrityResult begin "aM_message" of type CHOICE [UNIVERSAL 31] begin "uL_DCCH_Message" of type UL_DCCH_Message (SEQUENCE) [UNIVERSAL 16] begin "integrityCheckInfo" of type IntegrityCheckInfo (SEQUENCE) [UNIVERSAL 16] matching { messageAuthenticationCode: '11100000000110011010110001001011'B , rrc_MessageSequenceNumber: 2 } against * end "integrityCheckInfo" of type IntegrityCheckInfo begin "message" of type UL_DCCH_MessageType (CHOICE) [UNIVERSAL 31] begin "securityModeComplete" of type SecurityModeComplete (SEQUENCE) [UNIVERSAL 16] begin "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier (INTEGER) [UNIVERSAL 2] matching 0 against 0 end "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier begin "ul_IntegProtActivationInfo" of type IntegrityProtActivationInfo (SEQUENCE) [UNIVERSAL 16] matching { rrc_MessageSequenceNumberList: [ 5 , 1 , 2 , 3 , 1 ] } against * end "ul_IntegProtActivationInfo" of type IntegrityProtActivationInfo end "securityModeComplete" of type SecurityModeComplete end "message" of type UL_DCCH_MessageType end "uL_DCCH_Message" of type UL_DCCH_Message end "aM_message" of type CHOICE end "car_RRC_SecModeCmpl" of type RLC_AM_DATA_IND Assignment:TSP2: [34] uL_Integrity := { rrc_MessageSequenceNumberList: [ 5 , 1 , 2 , 3 , 1 ] } Receive event:TSP2: [34] AM ? RLC_AM_DATA_IND = PDU (view PDU) Preliminary verdict:TSP2: [34] (PASS) Attach:[35] Enter Test Step ts_CRLC_UL_Integrity( { rrc_MessageSequenceNumberList: [ 5 , 1 , 2 , 3 , 1 ] } )
| 00:03:29.630 - Primitive: CRLC_Integrity_Activate_REQ 00:03:29.630 - Primitive: CRLC_Integrity_Activate_REQ Send event:[1] CRLC ! CRLC_Integrity_Activate_REQ = PDU (view PDU) 00:03:29.650 - Primitive: CRLC_Integrity_Activate_CNF begin "ca_CRLC_IntegrityActivateCnf" of type CRLC_Integrity_Activate_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER end "ca_CRLC_IntegrityActivateCnf" of type CRLC_Integrity_Activate_CNF Receive event:[2] CRLC ? CRLC_Integrity_Activate_CNF = PDU: { cellId: -1 } Attach:[35] Exit Test Step ts_CRLC_UL_Integrity
Attach:[6] Exit Test Step ts_RRC_Security::lt_StartSecurity_UE
Attach:[2] Exit Test Step ts_RRC_Security
Attach:[39] Exit Test Step ts_GMM_AuthenticateAndStartIntegrityProtection
Assignment:[40] tcv_AssignedPTMSI := '12345678'O Assignment:[40] tcv_Assigned_PTMSI_Sig := 'AB1234'O 00:03:29.650 - Primitive: RRC_DATA_REQ: gmm:attachAccept 00:03:29.650 - Primitive: RLC_AM_DATA_REQ:downlinkDirectTransfer Send event:[40] Dc ! RRC_DataReq = PDU (view PDU) 00:03:29.930 - Primitive: RLC_AM_DATA_IND: uplinkDirectTransfer 00:03:29.930 - Primitive: RRC_DATA_IND: gmm:attachComplete begin "car_PS_UplinkDirectTransfer" of type RRC_DataInd (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "rB_Id" of type SS_RB_Identity (INTEGER) [UNIVERSAL 2] matching 3 against 3 end "rB_Id" of type SS_RB_Identity begin "cN_Domain" of type SS_CN_DomainIdentity (INTEGER) [UNIVERSAL 2] matching 1 against 1 end "cN_Domain" of type SS_CN_DomainIdentity begin "msg" of type ATTACHCOMPLETE (SEQUENCE) [UNIVERSAL 16] begin "skipIndicator" of type SkipIndicator (BITSTRING) [UNIVERSAL 3] matching '0000'B against '0000'B end "skipIndicator" of type SkipIndicator begin "gMMProtocolDiscriminator" of type ProtocolDiscriminator (BITSTRING) [UNIVERSAL 3] matching '1000'B against '1000'B end "gMMProtocolDiscriminator" of type ProtocolDiscriminator begin "msgType" of type MsgType (BITSTRING) [UNIVERSAL 3] matching '00000011'B against '00000011'B end "msgType" of type MsgType end "msg" of type ATTACHCOMPLETE end "car_PS_UplinkDirectTransfer" of type RRC_DataInd Receive event:[41] Dc ? RRC_DataInd = PDU (view PDU) Attach:[42] Enter Test Step ts_RRC_ConnRel( 3 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 3 )
| Assignment:[8] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[2] Enter Test Step ts_RRC_Delay( 1000 )
| StartTimer:[1] t_Dly [5000] 1000 ms Timed out Timer:t_Dly TimeOut:[2] t_Dly [5000] 1000 ms Attach:[2] Exit Test Step ts_RRC_Delay
Attach:[3] Enter Test Step ts_RRC_ConnRel::lt_Send_RRC_ConnectionRelease( 3 )
| Assignment:[39] tcv_N308 := 1 Assignment:[39] tcv_K := 1 00:03:30.960 - Primitive: RLC_UM_DATA_REQ 00:03:30.960 - Primitive: RLC_UM_DATA_REQ: rrcConnectionRelease Send event:[40] UM ! RLC_UM_DATA_REQ = PDU (view PDU) 00:03:31.230 - Primitive: RLC_UM_DATA_IND: rrcConnectionReleaseComplete 00:03:31.230 - Primitive: RLC_UM_DATA_IND begin "car_RRC_ConnRelCmplUM" of type RLC_UM_DATA_IND (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "integrityResult" of type IntegrityResult (CHOICE) [UNIVERSAL 31] matching [integrityUsed: i_pass] against * end "integrityResult" of type IntegrityResult begin "uM_message" of type CHOICE [UNIVERSAL 31] begin "uL_DCCH_Message" of type UL_DCCH_Message (SEQUENCE) [UNIVERSAL 16] begin "integrityCheckInfo" of type IntegrityCheckInfo (SEQUENCE) [UNIVERSAL 16] matching { messageAuthenticationCode: '11110111111000101100001011001110'B , rrc_MessageSequenceNumber: 1 } against * end "integrityCheckInfo" of type IntegrityCheckInfo begin "message" of type UL_DCCH_MessageType (CHOICE) [UNIVERSAL 31] begin "rrcConnectionReleaseComplete" of type RRCConnectionReleaseComplete (SEQUENCE) [UNIVERSAL 16] begin "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier (INTEGER) [UNIVERSAL 2] matching 0 against 0 end "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier end "rrcConnectionReleaseComplete" of type RRCConnectionReleaseComplete end "message" of type UL_DCCH_MessageType end "uL_DCCH_Message" of type UL_DCCH_Message end "uM_message" of type CHOICE end "car_RRC_ConnRelCmplUM" of type RLC_UM_DATA_IND Receive event:TSP1: [41] UM ? RLC_UM_DATA_IND = PDU (view PDU) Preliminary verdict:TSP1: [41] (PASS) Attach:[42] Enter Test Step ts_RRC_ConnRel::lt_RptRcvConnRel( 3 )
| StartTimer:[50] t_Dly [5000] 5000 ms 00:03:31.400 - Primitive: RLC_UM_DATA_IND: rrcConnectionReleaseComplete 00:03:31.400 - Primitive: RLC_UM_DATA_IND begin "car_RRC_ConnRelCmplUM" of type RLC_UM_DATA_IND (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "integrityResult" of type IntegrityResult (CHOICE) [UNIVERSAL 31] matching [integrityUsed: i_pass] against * end "integrityResult" of type IntegrityResult begin "uM_message" of type CHOICE [UNIVERSAL 31] begin "uL_DCCH_Message" of type UL_DCCH_Message (SEQUENCE) [UNIVERSAL 16] begin "integrityCheckInfo" of type IntegrityCheckInfo (SEQUENCE) [UNIVERSAL 16] matching { messageAuthenticationCode: '10111001101000110000011111000000'B , rrc_MessageSequenceNumber: 2 } against * end "integrityCheckInfo" of type IntegrityCheckInfo begin "message" of type UL_DCCH_MessageType (CHOICE) [UNIVERSAL 31] begin "rrcConnectionReleaseComplete" of type RRCConnectionReleaseComplete (SEQUENCE) [UNIVERSAL 16] begin "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier (INTEGER) [UNIVERSAL 2] matching 0 against 0 end "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier end "rrcConnectionReleaseComplete" of type RRCConnectionReleaseComplete end "message" of type UL_DCCH_MessageType end "uL_DCCH_Message" of type UL_DCCH_Message end "uM_message" of type CHOICE end "car_RRC_ConnRelCmplUM" of type RLC_UM_DATA_IND Assignment:TSP2: [53] tcv_K := 2 CancelTimer:TSP2: [53] t_Dly [5000] 5000 ms Receive event:TSP2: [53] UM ? RLC_UM_DATA_IND = PDU (view PDU) Preliminary verdict:TSP2: [53] (PASS) Attach:[42] Exit Test Step ts_RRC_ConnRel::lt_RptRcvConnRel
Attach:[3] Exit Test Step ts_RRC_ConnRel::lt_Send_RRC_ConnectionRelease
Attach:[4] Enter Test Step ts_RRC_ConnRel::lt_RestartCRLC_ForNextConnection( 3 )
| Attach:[7] Enter Test Step ts_CRLC_RelReconfSRB( 3 )
| Attach:[1] Enter Test Step ts_CRLC_Rel( -1 )
| 00:03:31.400 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:03:31.420 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 1 ]} Attach:[1] Exit Test Step ts_CRLC_Rel
Attach:[2] Enter Test Step ts_CRLC_Rel( -1 )
| 00:03:31.420 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:03:31.430 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 2 ]} Attach:[2] Exit Test Step ts_CRLC_Rel
Attach:[3] Enter Test Step ts_CRLC_Rel( -1 )
| 00:03:31.430 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:03:31.450 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 3 ]} Attach:[3] Exit Test Step ts_CRLC_Rel
Attach:[4] Enter Test Step ts_CRLC_Rel( -1 )
| 00:03:31.450 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:03:31.460 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 4 ]} Attach:[4] Exit Test Step ts_CRLC_Rel
Attach:[5] Enter Test Step ts_SS_RB1_ToRB4_Cfg( )
| 00:03:31.460 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:03:31.480 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 1 ]} 00:03:31.480 - Primitive: CRLC_Config_REQ Send event:[3] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:03:31.490 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[4] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 2 ]} 00:03:31.490 - Primitive: CRLC_Config_REQ Send event:[5] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:03:31.510 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[6] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 3 ]} 00:03:31.510 - Primitive: CRLC_Config_REQ Send event:[7] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:03:31.530 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[8] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 4 ]} Attach:[5] Exit Test Step ts_SS_RB1_ToRB4_Cfg
Attach:[7] Exit Test Step ts_CRLC_RelReconfSRB
Attach:[8] Enter Test Step ts_SetCellCfg( 3 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 3 )
| Assignment:[8] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Assignment:[2] cellConfig := cell_DCH_StandAloneSRB_NoConn Attach:[3] Enter Test Step ts_SaveCellInfo( 3 )
| Assignment:[8] tcv_CellInfoD := (view Assignment) Attach:[3] Exit Test Step ts_SaveCellInfo
Attach:[8] Exit Test Step ts_SetCellCfg
Attach:[4] Exit Test Step ts_RRC_ConnRel::lt_RestartCRLC_ForNextConnection
Attach:[5] Enter Test Step ts_SS_ResetSecurityKey( )
| Assignment:[1] tcv_CellIndInfo := (view Assignment) Assignment:[3] cipheringAlgorithmCapability := '0000000000000011'B Attach:[5] Exit Test Step ts_SS_ResetSecurityKey
Attach:[42] Exit Test Step ts_RRC_ConnRel
Attach:[25] Exit Test Step tc_12_4_1_2::lt_Attach_Steps_17To19
Attach:[26] Enter Test Step ts_GMM_DetachOnSwitchOff( 3 )
| Attach:[1] Enter Test Step ts_RRC_Delay( 5000 )
| StartTimer:[1] t_Dly [5000] 5000 ms Timed out Timer:t_Dly TimeOut:[2] t_Dly [5000] 5000 ms Attach:[1] Exit Test Step ts_RRC_Delay
Attach:[3] Enter Test Step ts_SetTmpCellInfo( 3 )
| Assignment:[8] tcv_TmpCellInfo := (view Assignment) Attach:[3] Exit Test Step ts_SetTmpCellInfo
Attach:[4] Enter Test Step ts_GMM_DetachOnSwitchOff::lt_Init_RRC_RelStatus( 3 )
| Assignment:[24] tcv_RRC_RelStatus := cell_Dch Attach:[4] Exit Test Step ts_GMM_DetachOnSwitchOff::lt_Init_RRC_RelStatus
Attach:[5] Enter Test Step ts_MMI_UE_SwitchOff( )
| 00:03:36.540 - Primitive: MMI_CmdReq Send event:[2] Ut ! MMI_CmdReq = PDU: { cmd: "Please switch off the UE" } 00:03:38.170 - Primitive: MMI_CmdCnf begin "ca_MMI_CmdCnf" of type MMI_CmdCnf (SEQUENCE) [UNIVERSAL 16] begin "result" of type BOOLEAN [UNIVERSAL 1] matching GcTRUE against GcTRUE end "result" of type BOOLEAN end "ca_MMI_CmdCnf" of type MMI_CmdCnf Receive event:[3] Ut ? MMI_CmdCnf = PDU: { result: GcTRUE , resultString: OMIT} Assignment:[4] tcv_UE_SwitchedOn := GcFALSE Attach:[5] Exit Test Step ts_MMI_UE_SwitchOff
Attach:[6] Enter Test Step ts_RRC_ConnEst( 3 )
| Attach:[1] Enter Test Step ts_SS_PrepareCellRRC_ConnEst( 3 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 3 )
| Assignment:[8] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[1] Exit Test Step ts_SS_PrepareCellRRC_ConnEst
Attach:[2] Enter Test Step ts_SetTmpCellInfo( 3 )
| Assignment:[8] tcv_TmpCellInfo := (view Assignment) Attach:[2] Exit Test Step ts_SetTmpCellInfo
Attach:[3] Enter Test Step ts_RRC_ConnEst::lt_RcvConnReq( 3 )
| 00:03:41.560 - Primitive: RLC_TR_DATA_IND: rrcConnectionRequest 00:03:41.560 - Primitive: RLC_TR_DATA_IND begin "car_RRC_ConnReq" of type RLC_TR_DATA_IND (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "tM_message" of type CHOICE [UNIVERSAL 31] begin "uL_CCCH_Message" of type UL_CCCH_Message (SEQUENCE) [UNIVERSAL 16] begin "message" of type UL_CCCH_MessageType (CHOICE) [UNIVERSAL 31] begin "rrcConnectionRequest" of type RRCConnectionRequest (SEQUENCE) [UNIVERSAL 16] begin "initialUE_Identity" of type InitialUE_Identity (CHOICE) [UNIVERSAL 31] begin InitialUE_Identity (CHOICE) [UNIVERSAL 31] end InitialUE_Identity begin InitialUE_Identity (CHOICE) [UNIVERSAL 31] begin "tmsi_and_LAI" of type TMSI_and_LAI_GSM_MAP (SEQUENCE) [UNIVERSAL 16] matching { tmsi: '00010001001000100011001101000100'B , lai: { plmn_Identity: { mcc: [ 0 , 0 , 2 ] , mnc: [ 0 , 1 ] } , lac: '0000000000000001'B } } against ? end "tmsi_and_LAI" of type TMSI_and_LAI_GSM_MAP end InitialUE_Identity matching [tmsi_and_LAI: { tmsi: '00010001001000100011001101000100'B , lai: { plmn_Identity: { mcc: [ 0 , 0 , 2 ] , mnc: [ 0 , 1 ] } , lac: '0000000000000001'B } } ] against ([imsi: ?], [tmsi_and_LAI: ?], [p_TMSI_and_RAI: ?], [imei: ?]) end "initialUE_Identity" of type InitialUE_Identity begin "establishmentCause" of type EstablishmentCause (ENUMERATED) [UNIVERSAL 10] matching detach against detach end "establishmentCause" of type EstablishmentCause begin "protocolErrorIndicator" of type ProtocolErrorIndicator (ENUMERATED) [UNIVERSAL 10] matching noError against noError end "protocolErrorIndicator" of type ProtocolErrorIndicator end "rrcConnectionRequest" of type RRCConnectionRequest end "message" of type UL_CCCH_MessageType end "uL_CCCH_Message" of type UL_CCCH_Message end "tM_message" of type CHOICE end "car_RRC_ConnReq" of type RLC_TR_DATA_IND Assignment:[9] tcv_InitialUE_Id := (view Assignment) Receive event:[9] TM ? RLC_TR_DATA_IND = PDU (view PDU) Attach:[3] Exit Test Step ts_RRC_ConnEst::lt_RcvConnReq
Attach:[4] Enter Test Step ts_RRC_ConnEst::lt_Send_ConnSetUp( 3 )
| 00:03:41.560 - Primitive: RLC_UM_DATA_REQ 00:03:41.560 - Primitive: RLC_UM_DATA_REQ: rrcConnectionSetup Send event:[31] UM ! RLC_UM_DATA_REQ = PDU (view PDU) Attach:[33] Enter Test Step ts_SetCellCfg( 3 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 3 )
| Assignment:[8] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Assignment:[2] cellConfig := cell_DCH_StandAloneSRB Attach:[3] Enter Test Step ts_SaveCellInfo( 3 )
| Assignment:[8] tcv_CellInfoD := (view Assignment) Attach:[3] Exit Test Step ts_SaveCellInfo
Attach:[33] Exit Test Step ts_SetCellCfg
Attach:[4] Exit Test Step ts_RRC_ConnEst::lt_Send_ConnSetUp
Attach:[5] Enter Test Step ts_RRC_ReceiveConnSetupCmpl( 3 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 3 )
| Assignment:[8] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
StartTimer:[3] t_WaitMS [13500] 13500 ms 00:03:42.060 - Primitive: RLC_AM_DATA_IND: rrcConnectionSetupComplete 00:03:42.060 - Primitive: RLC_AM_DATA_IND begin "car_RRC_ConnSetupCmpl" of type RLC_AM_DATA_IND (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "integrityResult" of type IntegrityResult (CHOICE) [UNIVERSAL 31] matching [integrityUsed: i_pass] against ? end "integrityResult" of type IntegrityResult begin "aM_message" of type CHOICE [UNIVERSAL 31] begin "uL_DCCH_Message" of type UL_DCCH_Message (SEQUENCE) [UNIVERSAL 16] begin "message" of type UL_DCCH_MessageType (CHOICE) [UNIVERSAL 31] begin "rrcConnectionSetupComplete" of type RRCConnectionSetupComplete (SEQUENCE) [UNIVERSAL 16] begin "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier (INTEGER) [UNIVERSAL 2] matching 0 against 0 end "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier begin "startList" of type STARTList (SEQUENCEOF) [UNIVERSAL 28] matching [ { cn_DomainIdentity: ps_domain, start_Value: '00000000000000000010'B } , { cn_DomainIdentity: cs_domain, start_Value: '00000000000000000010'B } ] against ? end "startList" of type STARTList begin "ue_RadioAccessCapability" of type UE_RadioAccessCapability (SEQUENCE) [UNIVERSAL 16] matching { accessStratumReleaseIndicator: r99, pdcp_Capability: { losslessSRNS_RelocationSupport: GcFALSE , supportForRfc2507: [notSupported: NULL]} , rlc_Capability: { totalRLC_AM_BufferSize: kb50, maximumRLC_WindowSize: mws2047, maximumAM_EntityNumber: am6} , transportChannelCapability: { dl_TransChCapability: { maxNoBitsReceived: b8960, maxConvCodeBitsReceived: b1280, turboDecodingSupport: [supported: b8960], maxSimultaneousTransChs: e8, maxSimultaneousCCTrCH_Count: 1 , maxReceivedTransportBlocks: tb32, maxNumberOfTFC: tfc128, maxNumberOfTF: tf64} , ul_TransChCapability: { maxNoBitsTransmitted: b3840, maxConvCodeBitsTransmitted: b1280, turboEncodingSupport: [supported: b3840], maxSimultaneousTransChs: e8, modeSpecificInfo: [fdd: NULL], maxTransmittedBlocks: tb32, maxNumberOfTFC: tfc64, maxNumberOfTF: tf32} } , rf_Capability: { fddRF_Capability: { ue_PowerClass: 4 , txRxFrequencySeparation: mhz190} , tddRF_Capability: OMIT} , physicalChannelCapability: { fddPhysChCapability: { downlinkPhysChCapability: { maxNoDPCH_PDSCH_Codes: 1 , maxNoPhysChBitsReceived: b9600, supportForSF_512: GcFALSE , supportOfPDSCH: GcFALSE , simultaneousSCCPCH_DPCH_Reception: [notSupported: NULL]} , uplinkPhysChCapability: { maxNoDPDCH_BitsTransmitted: b4800, supportOfPCPCH: GcFALSE } } , tddPhysChCapability: OMIT} , ue_MultiModeRAT_Capability: { multiRAT_CapabilityList: { supportOfGSM: GcFALSE , supportOfMulticarrier: GcFALSE } , multiModeCapability: fdd} , securityCapability: { cipheringAlgorithmCap: '0000000000000011'B , integrityProtectionAlgorithmCap: '0000000000000010'B } , ue_positioning_Capability: { standaloneLocMethodsSupported: GcFALSE , ue_BasedOTDOA_Supported: GcFALSE , networkAssistedGPS_Supported: noNetworkAssistedGPS, supportForUE_GPS_TimingOfCellFrames: GcFALSE , supportForIPDL: GcFALSE } , measurementCapability: { downlinkCompressedMode: { fdd_Measurements: GcTRUE , tdd_Measurements: OMIT, gsm_Measurements: { gsm900: GcTRUE , dcs1800: GcTRUE , gsm1900: GcTRUE } , multiCarrierMeasurements: GcFALSE } , uplinkCompressedMode: { fdd_Measurements: GcTRUE , tdd_Measurements: OMIT, gsm_Measurements: { gsm900: GcTRUE , dcs1800: GcTRUE , gsm1900: GcTRUE } , multiCarrierMeasurements: GcFALSE } } } against * end "ue_RadioAccessCapability" of type UE_RadioAccessCapability end "rrcConnectionSetupComplete" of type RRCConnectionSetupComplete end "message" of type UL_DCCH_MessageType end "uL_DCCH_Message" of type UL_DCCH_Message end "aM_message" of type CHOICE end "car_RRC_ConnSetupCmpl" of type RLC_AM_DATA_IND Assignment:TSP1: [5] tcv_StartList := (view Assignment) Assignment:TSP1: [5] cipheringAlgorithmCapability := '0000000000000011'B CancelTimer:TSP1: [5] t_WaitMS [13500] 13500 ms Receive event:TSP1: [5] AM ? RLC_AM_DATA_IND = PDU (view PDU) Preliminary verdict:TSP1: [5] (PASS) Attach:[6] Enter Test Step ts_RRC_ReceiveConnSetupCmpl::lt_GetHFN( 3 )
| Assignment:[13] tcv_Count := 2 Attach:[17] Enter Test Step ts_RRC_ReceiveConnSetupCmpl::lt_FirstValue( 3 )
| Assignment:[23] start_PS := '00000000000000000010'B Attach:[17] Exit Test Step ts_RRC_ReceiveConnSetupCmpl::lt_FirstValue
Attach:[18] Enter Test Step ts_RRC_ReceiveConnSetupCmpl::lt_SecondValue( 3 )
| Assignment:[26] start_CS := '00000000000000000010'B Attach:[18] Exit Test Step ts_RRC_ReceiveConnSetupCmpl::lt_SecondValue
Attach:[6] Exit Test Step ts_RRC_ReceiveConnSetupCmpl::lt_GetHFN
Attach:[5] Exit Test Step ts_RRC_ReceiveConnSetupCmpl
Attach:[6] Exit Test Step ts_RRC_ConnEst
Attach:[8] Enter Test Step ts_GMM_DetachOnSwitchOff::lt_Detach_PSonly( 3 )
| Attach:[8] Exit Test Step ts_GMM_DetachOnSwitchOff::lt_Detach_PSonly
00:03:42.070 - Primitive: RLC_AM_DATA_IND: initialDirectTransfer 00:03:42.070 - Primitive: RRC_DATA_IND: gmm:detachRequest Attach:[8] Enter Test Step ts_GMM_DetachOnSwitchOff::lt_Detach_PSonly( 3 )
| begin "car_PS_InitDirectTransfer" of type RRC_DataInd (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "rB_Id" of type SS_RB_Identity (INTEGER) [UNIVERSAL 2] matching 3 against 3 end "rB_Id" of type SS_RB_Identity begin "cN_Domain" of type SS_CN_DomainIdentity (INTEGER) [UNIVERSAL 2] matching 1 against 1 end "cN_Domain" of type SS_CN_DomainIdentity begin "start" of type START_Value (BITSTRING) [UNIVERSAL 3] matching '00000000000000000010'B against ? end "start" of type START_Value begin "msg" of type DETACHREQUESTMO (SEQUENCE) [UNIVERSAL 16] begin "skipIndicator" of type SkipIndicator (BITSTRING) [UNIVERSAL 3] matching '0000'B against '0000'B end "skipIndicator" of type SkipIndicator begin "gMMProtocolDiscriminator" of type ProtocolDiscriminator (BITSTRING) [UNIVERSAL 3] matching '1000'B against '1000'B end "gMMProtocolDiscriminator" of type ProtocolDiscriminator begin "msgType" of type MsgType (BITSTRING) [UNIVERSAL 3] matching '00000101'B against '00000101'B end "msgType" of type MsgType begin "spare4" of type B4 (BITSTRING) [UNIVERSAL 3] matching '0000'B against ? end "spare4" of type B4 begin "detachType" of type DetachType (SEQUENCE) [UNIVERSAL 16] begin "powOff" of type B1 (BITSTRING) [UNIVERSAL 3] matching '1'B against '1'B end "powOff" of type B1 begin "type" of type B3 (BITSTRING) [UNIVERSAL 3] matching '001'B against '001'B end "type" of type B3 end "detachType" of type DetachType begin "ptmsi" of type GMM_MS_IdentityPTMSI (SEQUENCE) [UNIVERSAL 16] begin "iei" of type IEI8 (BITSTRING) [UNIVERSAL 3] matching '00011000'B against '00011000'B end "iei" of type IEI8 begin "iel" of type Length (OCTETSTRING) [UNIVERSAL 4] matching '05'O against '05'O end "iel" of type Length begin "iDigit1" of type B4 (BITSTRING) [UNIVERSAL 3] matching '1111'B against '1111'B end "iDigit1" of type B4 begin "oddEvenInd" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against '0'B end "oddEvenInd" of type B1 begin "typeOfId" of type B3 (BITSTRING) [UNIVERSAL 3] matching '100'B against '100'B end "typeOfId" of type B3 begin "otherDigits" of type OCTETSTRING [UNIVERSAL 4] matching '12345678'O against '12345678'O end "otherDigits" of type OCTETSTRING end "ptmsi" of type GMM_MS_IdentityPTMSI begin "ptmsiSignature" of type PTMSI_Signature_tlv (SEQUENCE) [UNIVERSAL 16] begin "iei" of type IEI8 (BITSTRING) [UNIVERSAL 3] matching '00011001'B against '00011001'B end "iei" of type IEI8 begin "iel" of type Length (OCTETSTRING) [UNIVERSAL 4] matching '03'O against '03'O end "iel" of type Length begin "value" of type OCTETSTRING [UNIVERSAL 4] matching 'AB1234'O against 'AB1234'O end "value" of type OCTETSTRING end "ptmsiSignature" of type PTMSI_Signature_tlv end "msg" of type DETACHREQUESTMO end "car_PS_InitDirectTransfer" of type RRC_DataInd Receive event:[26] Dc ? RRC_DataInd = PDU (view PDU) Preliminary verdict:[26] (PASS) Attach:[8] Exit Test Step ts_GMM_DetachOnSwitchOff::lt_Detach_PSonly
Attach:[9] Enter Test Step ts_RRC_ConnRel_AfterSwitchOff( 3 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 3 )
| Assignment:[8] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[2] Enter Test Step ts_RRC_Delay( 1000 )
| StartTimer:[1] t_Dly [5000] 1000 ms Timed out Timer:t_Dly TimeOut:[2] t_Dly [5000] 1000 ms Attach:[2] Exit Test Step ts_RRC_Delay
Attach:[3] Enter Test Step ts_RRC_ConnRel_AfterSwitchOff::lt_Send_RRC_ConnectionRelease( 3 )
| Assignment:[39] tcv_N308 := 1 Assignment:[39] tcv_K := 1 00:03:43.100 - Primitive: RLC_UM_DATA_REQ 00:03:43.100 - Primitive: RLC_UM_DATA_REQ: rrcConnectionRelease Send event:[40] UM ! RLC_UM_DATA_REQ = PDU (view PDU) StartTimer:[41] t_Dly [5000] 1000 ms 00:03:43.370 - Primitive: RLC_UM_DATA_IND: rrcConnectionReleaseComplete 00:03:43.370 - Primitive: RLC_UM_DATA_IND begin "car_RRC_ConnRelCmplUM" of type RLC_UM_DATA_IND (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "integrityResult" of type IntegrityResult (CHOICE) [UNIVERSAL 31] matching [integrityUsed: i_pass] against * end "integrityResult" of type IntegrityResult begin "uM_message" of type CHOICE [UNIVERSAL 31] begin "uL_DCCH_Message" of type UL_DCCH_Message (SEQUENCE) [UNIVERSAL 16] begin "message" of type UL_DCCH_MessageType (CHOICE) [UNIVERSAL 31] begin "rrcConnectionReleaseComplete" of type RRCConnectionReleaseComplete (SEQUENCE) [UNIVERSAL 16] begin "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier (INTEGER) [UNIVERSAL 2] matching 0 against 0 end "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier end "rrcConnectionReleaseComplete" of type RRCConnectionReleaseComplete end "message" of type UL_DCCH_MessageType end "uL_DCCH_Message" of type UL_DCCH_Message end "uM_message" of type CHOICE end "car_RRC_ConnRelCmplUM" of type RLC_UM_DATA_IND CancelTimer:TSP1: [43] t_Dly [5000] 1000 ms Receive event:TSP1: [43] UM ? RLC_UM_DATA_IND = PDU (view PDU) Preliminary verdict:TSP1: [43] (PASS) Attach:[44] Enter Test Step ts_RRC_ConnRel_AfterSwitchOff::lt_RptRcvConnRel( 3 )
| StartTimer:[54] t_Dly [5000] 5000 ms 00:03:43.540 - Primitive: RLC_UM_DATA_IND: rrcConnectionReleaseComplete 00:03:43.540 - Primitive: RLC_UM_DATA_IND begin "car_RRC_ConnRelCmplUM" of type RLC_UM_DATA_IND (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "integrityResult" of type IntegrityResult (CHOICE) [UNIVERSAL 31] matching [integrityUsed: i_pass] against * end "integrityResult" of type IntegrityResult begin "uM_message" of type CHOICE [UNIVERSAL 31] begin "uL_DCCH_Message" of type UL_DCCH_Message (SEQUENCE) [UNIVERSAL 16] begin "message" of type UL_DCCH_MessageType (CHOICE) [UNIVERSAL 31] begin "rrcConnectionReleaseComplete" of type RRCConnectionReleaseComplete (SEQUENCE) [UNIVERSAL 16] begin "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier (INTEGER) [UNIVERSAL 2] matching 0 against 0 end "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier end "rrcConnectionReleaseComplete" of type RRCConnectionReleaseComplete end "message" of type UL_DCCH_MessageType end "uL_DCCH_Message" of type UL_DCCH_Message end "uM_message" of type CHOICE end "car_RRC_ConnRelCmplUM" of type RLC_UM_DATA_IND Assignment:TSP2: [57] tcv_K := 2 CancelTimer:TSP2: [57] t_Dly [5000] 5000 ms Receive event:TSP2: [57] UM ? RLC_UM_DATA_IND = PDU (view PDU) Preliminary verdict:TSP2: [57] (PASS) Attach:[44] Exit Test Step ts_RRC_ConnRel_AfterSwitchOff::lt_RptRcvConnRel
Attach:[3] Exit Test Step ts_RRC_ConnRel_AfterSwitchOff::lt_Send_RRC_ConnectionRelease
Attach:[4] Enter Test Step ts_RRC_ConnRel_AfterSwitchOff::lt_RestartCRLC_ForNextConnection( 3 )
| Attach:[7] Enter Test Step ts_CRLC_RelReconfSRB( 3 )
| Attach:[1] Enter Test Step ts_CRLC_Rel( -1 )
| 00:03:43.540 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:03:43.560 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 1 ]} Attach:[1] Exit Test Step ts_CRLC_Rel
Attach:[2] Enter Test Step ts_CRLC_Rel( -1 )
| 00:03:43.560 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:03:43.570 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 2 ]} Attach:[2] Exit Test Step ts_CRLC_Rel
Attach:[3] Enter Test Step ts_CRLC_Rel( -1 )
| 00:03:43.570 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:03:43.590 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 3 ]} Attach:[3] Exit Test Step ts_CRLC_Rel
Attach:[4] Enter Test Step ts_CRLC_Rel( -1 )
| 00:03:43.590 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:03:43.600 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 4 ]} Attach:[4] Exit Test Step ts_CRLC_Rel
Attach:[5] Enter Test Step ts_SS_RB1_ToRB4_Cfg( )
| 00:03:43.600 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:03:43.620 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 1 ]} 00:03:43.620 - Primitive: CRLC_Config_REQ Send event:[3] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:03:43.630 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[4] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 2 ]} 00:03:43.630 - Primitive: CRLC_Config_REQ Send event:[5] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:03:43.650 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[6] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 3 ]} 00:03:43.650 - Primitive: CRLC_Config_REQ Send event:[7] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:03:43.670 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[8] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 4 ]} Attach:[5] Exit Test Step ts_SS_RB1_ToRB4_Cfg
Attach:[7] Exit Test Step ts_CRLC_RelReconfSRB
Attach:[8] Enter Test Step ts_SetCellCfg( 3 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 3 )
| Assignment:[8] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Assignment:[2] cellConfig := cell_DCH_StandAloneSRB_NoConn Attach:[3] Enter Test Step ts_SaveCellInfo( 3 )
| Assignment:[8] tcv_CellInfoD := (view Assignment) Attach:[3] Exit Test Step ts_SaveCellInfo
Attach:[8] Exit Test Step ts_SetCellCfg
Attach:[4] Exit Test Step ts_RRC_ConnRel_AfterSwitchOff::lt_RestartCRLC_ForNextConnection
Attach:[5] Enter Test Step ts_SS_ResetSecurityKey( )
| Assignment:[1] tcv_CellIndInfo := (view Assignment) Assignment:[3] cipheringAlgorithmCapability := '0000000000000011'B Attach:[5] Exit Test Step ts_SS_ResetSecurityKey
Attach:[9] Exit Test Step ts_RRC_ConnRel_AfterSwitchOff
Attach:[26] Exit Test Step ts_GMM_DetachOnSwitchOff
Attach:[10] Exit Test Step tc_12_4_1_2::lt_TestBody
Attach:[11] Enter Test Step po_ConnectionAndSS_Rels( )
| Attach:[1] Enter Test Step po_ConnectionAndSS_Rels::lt_ReleaseCell( 0 )
| Attach:[9] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[9] Exit Test Step ts_SetTmpCellInfo
Attach:[1] Exit Test Step po_ConnectionAndSS_Rels::lt_ReleaseCell
Attach:[2] Enter Test Step po_ConnectionAndSS_Rels::lt_ReleaseCell( 1 )
| Attach:[9] Enter Test Step ts_SetTmpCellInfo( 1 )
| Assignment:[4] tcv_TmpCellInfo := (view Assignment) Attach:[9] Exit Test Step ts_SetTmpCellInfo
Attach:[11] Enter Test Step po_ConnectionAndSS_Rel( 1 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 1 )
| Assignment:[4] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[3] Enter Test Step po_ConnectionAndSS_Rel::lt_Send_RRC_ConnectionRelease( 1 )
| Attach:[3] Exit Test Step po_ConnectionAndSS_Rel::lt_Send_RRC_ConnectionRelease
Attach:[4] Enter Test Step ts_SS_Rel( 1 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 1 )
| Assignment:[4] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[8] Enter Test Step ts_SS_Rel::lt_ReleaseCommonCh( 1 )
| Attach:[322] Enter Test Step ts_CRLC_Rel( 1 )
| 00:03:43.670 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:03:43.680 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: 1 , routingInfo: [rB_Identity: 0 ]} Attach:[322] Exit Test Step ts_CRLC_Rel
Attach:[323] Enter Test Step ts_CMAC_Rel( 1 )
| 00:03:43.680 - Primitive: CMAC_Config_REQ Send event:[1] CMAC ! CMAC_Config_REQ = PDU (view PDU) 00:03:43.700 - Primitive: CMAC_Config_CNF begin "ca_CMAC_CfgCnf" of type CMAC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 8 against 8 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_CfgCnf" of type CMAC_Config_CNF Receive event:[2] CMAC ? CMAC_Config_CNF = PDU: { cellId: 1 , routingInfo: [physicalChannelIdentity: 8 ]} Attach:[323] Exit Test Step ts_CMAC_Rel
Attach:[324] Enter Test Step ts_CPHY_TrChRelNonDch( 1 )
| 00:03:43.700 - Primitive: CPHY_TrCH_Release_REQ Send event:[1] CPHY ! CPHY_TrCH_Release_REQ = PDU (view PDU) 00:03:43.710 - Primitive: CPHY_TrCH_Release_CNF begin "ca_PHY_RelCnf" of type CPHY_TrCH_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 8 against 8 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_PHY_RelCnf" of type CPHY_TrCH_Release_CNF Receive event:[2] CPHY ? CPHY_TrCH_Release_CNF = PDU (view PDU) Attach:[324] Exit Test Step ts_CPHY_TrChRelNonDch
Attach:[325] Enter Test Step ts_SS_StopRL( 1 )
| 00:03:43.710 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 1 , routingInfo: [physicalChannelIdentity: 7 ]} 00:03:43.730 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 7 against 7 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 1 , routingInfo: [physicalChannelIdentity: 7 ]} Attach:[325] Exit Test Step ts_SS_StopRL
Attach:[326] Enter Test Step ts_SS_StopRL( 1 )
| 00:03:43.730 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 1 , routingInfo: [physicalChannelIdentity: 8 ]} 00:03:43.740 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 8 against 8 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 1 , routingInfo: [physicalChannelIdentity: 8 ]} Attach:[326] Exit Test Step ts_SS_StopRL
Attach:[327] Enter Test Step ts_CRLC_Rel( 1 )
| 00:03:43.740 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:03:43.760 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -2 against -2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: 1 , routingInfo: [rB_Identity: -2 ]} Attach:[327] Exit Test Step ts_CRLC_Rel
Attach:[328] Enter Test Step ts_CMAC_Rel( 1 )
| 00:03:43.760 - Primitive: CMAC_Config_REQ Send event:[1] CMAC ! CMAC_Config_REQ = PDU (view PDU) 00:03:43.780 - Primitive: CMAC_Config_CNF begin "ca_CMAC_CfgCnf" of type CMAC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 5 against 5 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_CfgCnf" of type CMAC_Config_CNF Receive event:[2] CMAC ? CMAC_Config_CNF = PDU: { cellId: 1 , routingInfo: [physicalChannelIdentity: 5 ]} Attach:[328] Exit Test Step ts_CMAC_Rel
Attach:[329] Enter Test Step ts_CPHY_TrChRelNonDch( 1 )
| 00:03:43.780 - Primitive: CPHY_TrCH_Release_REQ Send event:[1] CPHY ! CPHY_TrCH_Release_REQ = PDU (view PDU) 00:03:43.790 - Primitive: CPHY_TrCH_Release_CNF begin "ca_PHY_RelCnf" of type CPHY_TrCH_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 5 against 5 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_PHY_RelCnf" of type CPHY_TrCH_Release_CNF Receive event:[2] CPHY ? CPHY_TrCH_Release_CNF = PDU (view PDU) Attach:[329] Exit Test Step ts_CPHY_TrChRelNonDch
Attach:[330] Enter Test Step ts_SS_StopRL( 1 )
| 00:03:43.790 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 1 , routingInfo: [physicalChannelIdentity: 6 ]} 00:03:43.810 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 1 , routingInfo: [physicalChannelIdentity: 6 ]} Attach:[330] Exit Test Step ts_SS_StopRL
Attach:[331] Enter Test Step ts_SS_StopRL( 1 )
| 00:03:43.810 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 1 , routingInfo: [physicalChannelIdentity: 5 ]} 00:03:43.820 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 5 against 5 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 1 , routingInfo: [physicalChannelIdentity: 5 ]} Attach:[331] Exit Test Step ts_SS_StopRL
Attach:[8] Exit Test Step ts_SS_Rel::lt_ReleaseCommonCh
Attach:[9] Enter Test Step ts_SS_Rel::lt_Release_BCCH( 1 )
| Attach:[315] Enter Test Step ts_CRLC_Rel( 1 )
| 00:03:43.820 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:03:43.840 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: 1 , routingInfo: [rB_Identity: -1 ]} Attach:[315] Exit Test Step ts_CRLC_Rel
Attach:[316] Enter Test Step ts_CMAC_Rel( 1 )
| 00:03:43.840 - Primitive: CMAC_Config_REQ Send event:[1] CMAC ! CMAC_Config_REQ = PDU (view PDU) 00:03:43.850 - Primitive: CMAC_Config_CNF begin "ca_CMAC_CfgCnf" of type CMAC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_CfgCnf" of type CMAC_Config_CNF Receive event:[2] CMAC ? CMAC_Config_CNF = PDU: { cellId: 1 , routingInfo: [physicalChannelIdentity: 4 ]} Attach:[316] Exit Test Step ts_CMAC_Rel
Attach:[317] Enter Test Step ts_CPHY_TrChRelNonDch( 1 )
| 00:03:43.850 - Primitive: CPHY_TrCH_Release_REQ Send event:[1] CPHY ! CPHY_TrCH_Release_REQ = PDU (view PDU) 00:03:43.870 - Primitive: CPHY_TrCH_Release_CNF begin "ca_PHY_RelCnf" of type CPHY_TrCH_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_PHY_RelCnf" of type CPHY_TrCH_Release_CNF Receive event:[2] CPHY ? CPHY_TrCH_Release_CNF = PDU (view PDU) Attach:[317] Exit Test Step ts_CPHY_TrChRelNonDch
Attach:[318] Enter Test Step ts_SS_StopRL( 1 )
| 00:03:43.870 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 1 , routingInfo: [physicalChannelIdentity: 2 ]} 00:03:43.880 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 1 , routingInfo: [physicalChannelIdentity: 2 ]} Attach:[318] Exit Test Step ts_SS_StopRL
Attach:[319] Enter Test Step ts_SS_StopRL( 1 )
| 00:03:43.880 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 1 , routingInfo: [physicalChannelIdentity: 1 ]} 00:03:43.900 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 1 , routingInfo: [physicalChannelIdentity: 1 ]} Attach:[319] Exit Test Step ts_SS_StopRL
Attach:[320] Enter Test Step ts_SS_StopRL( 1 )
| 00:03:43.900 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 1 , routingInfo: [physicalChannelIdentity: 4 ]} 00:03:43.920 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 1 , routingInfo: [physicalChannelIdentity: 4 ]} Attach:[320] Exit Test Step ts_SS_StopRL
Attach:[321] Enter Test Step ts_SS_StopRL( 1 )
| 00:03:43.920 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 1 , routingInfo: [physicalChannelIdentity: 0 ]} 00:03:43.930 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 1 , routingInfo: [physicalChannelIdentity: 0 ]} Attach:[321] Exit Test Step ts_SS_StopRL
Attach:[9] Exit Test Step ts_SS_Rel::lt_Release_BCCH
Attach:[10] Enter Test Step ts_SetCellCfg( 1 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 1 )
| Assignment:[4] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Assignment:[2] cellConfig := cell_NotConfigured Attach:[3] Enter Test Step ts_SaveCellInfo( 1 )
| Assignment:[4] tcv_CellInfoB := (view Assignment) Attach:[3] Exit Test Step ts_SaveCellInfo
Attach:[10] Exit Test Step ts_SetCellCfg
Attach:[4] Exit Test Step ts_SS_Rel
Attach:[11] Exit Test Step po_ConnectionAndSS_Rel
Attach:[2] Exit Test Step po_ConnectionAndSS_Rels::lt_ReleaseCell
Attach:[3] Enter Test Step po_ConnectionAndSS_Rels::lt_ReleaseCell( 2 )
| Attach:[9] Enter Test Step ts_SetTmpCellInfo( 2 )
| Assignment:[6] tcv_TmpCellInfo := (view Assignment) Attach:[9] Exit Test Step ts_SetTmpCellInfo
Attach:[3] Exit Test Step po_ConnectionAndSS_Rels::lt_ReleaseCell
Attach:[4] Enter Test Step po_ConnectionAndSS_Rels::lt_ReleaseCell( 3 )
| Attach:[9] Enter Test Step ts_SetTmpCellInfo( 3 )
| Assignment:[8] tcv_TmpCellInfo := (view Assignment) Attach:[9] Exit Test Step ts_SetTmpCellInfo
Attach:[11] Enter Test Step po_ConnectionAndSS_Rel( 3 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 3 )
| Assignment:[8] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[3] Enter Test Step po_ConnectionAndSS_Rel::lt_Send_RRC_ConnectionRelease( 3 )
| Attach:[3] Exit Test Step po_ConnectionAndSS_Rel::lt_Send_RRC_ConnectionRelease
Attach:[4] Enter Test Step ts_SS_Rel( 3 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 3 )
| Assignment:[8] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[3] Enter Test Step ts_SS_RelDPCH( 3 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 3 )
| Assignment:[8] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[3] Enter Test Step ts_SS_RelDPCH::lt_RelSRB1_4( 3 )
| Attach:[119] Enter Test Step ts_CRLC_Rel( -1 )
| 00:03:43.930 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:03:43.950 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 1 ]} Attach:[119] Exit Test Step ts_CRLC_Rel
Attach:[120] Enter Test Step ts_CRLC_Rel( -1 )
| 00:03:43.950 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:03:43.960 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 2 ]} Attach:[120] Exit Test Step ts_CRLC_Rel
Attach:[121] Enter Test Step ts_CRLC_Rel( -1 )
| 00:03:43.960 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:03:43.980 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 3 ]} Attach:[121] Exit Test Step ts_CRLC_Rel
Attach:[122] Enter Test Step ts_CRLC_Rel( -1 )
| 00:03:43.980 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:03:43.990 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 4 ]} Attach:[122] Exit Test Step ts_CRLC_Rel
Attach:[3] Exit Test Step ts_SS_RelDPCH::lt_RelSRB1_4
Attach:[4] Enter Test Step ts_CMAC_Rel( -1 )
| 00:03:43.990 - Primitive: CMAC_Config_REQ Send event:[1] CMAC ! CMAC_Config_REQ = PDU (view PDU) 00:03:44.030 - Primitive: CMAC_Config_CNF begin "ca_CMAC_CfgCnf" of type CMAC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 26 against 26 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_CfgCnf" of type CMAC_Config_CNF Receive event:[2] CMAC ? CMAC_Config_CNF = PDU: { cellId: -1 , routingInfo: [physicalChannelIdentity: 26 ]} Attach:[4] Exit Test Step ts_CMAC_Rel
Attach:[5] Enter Test Step ts_CMAC_Rel( -1 )
| 00:03:44.030 - Primitive: CMAC_Config_REQ Send event:[1] CMAC ! CMAC_Config_REQ = PDU (view PDU) 00:03:44.070 - Primitive: CMAC_Config_CNF begin "ca_CMAC_CfgCnf" of type CMAC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 20 against 20 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_CfgCnf" of type CMAC_Config_CNF Receive event:[2] CMAC ? CMAC_Config_CNF = PDU: { cellId: -1 , routingInfo: [physicalChannelIdentity: 20 ]} Attach:[5] Exit Test Step ts_CMAC_Rel
Attach:[6] Enter Test Step ts_CPHY_TrChRelDCH_NoSHO( 3 )
| 00:03:44.070 - Primitive: CPHY_TrCH_Release_REQ Send event:[1] CPHY ! CPHY_TrCH_Release_REQ = PDU (view PDU) 00:03:44.090 - Primitive: CPHY_TrCH_Release_CNF begin "ca_PHY_RelCnf" of type CPHY_TrCH_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 26 against 26 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_PHY_RelCnf" of type CPHY_TrCH_Release_CNF Receive event:[2] CPHY ? CPHY_TrCH_Release_CNF = PDU (view PDU) Attach:[6] Exit Test Step ts_CPHY_TrChRelDCH_NoSHO
Attach:[7] Enter Test Step ts_CPHY_TrChRelDCH_NoSHO( 3 )
| 00:03:44.090 - Primitive: CPHY_TrCH_Release_REQ Send event:[1] CPHY ! CPHY_TrCH_Release_REQ = PDU (view PDU) 00:03:44.100 - Primitive: CPHY_TrCH_Release_CNF begin "ca_PHY_RelCnf" of type CPHY_TrCH_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 20 against 20 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_PHY_RelCnf" of type CPHY_TrCH_Release_CNF Receive event:[2] CPHY ? CPHY_TrCH_Release_CNF = PDU (view PDU) Attach:[7] Exit Test Step ts_CPHY_TrChRelDCH_NoSHO
Attach:[8] Enter Test Step ts_SS_StopRL( 3 )
| 00:03:44.100 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 26 ]} 00:03:44.120 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 26 against 26 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 26 ]} Attach:[8] Exit Test Step ts_SS_StopRL
Attach:[9] Enter Test Step ts_SS_StopRL( 3 )
| 00:03:44.120 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 20 ]} 00:03:44.130 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 20 against 20 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 20 ]} Attach:[9] Exit Test Step ts_SS_StopRL
Attach:[3] Exit Test Step ts_SS_RelDPCH
Attach:[4] Enter Test Step ts_SS_Rel::lt_ReleaseCommonCh( 3 )
| Attach:[322] Enter Test Step ts_CRLC_Rel( 3 )
| 00:03:44.130 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:03:44.150 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: 0 ]} Attach:[322] Exit Test Step ts_CRLC_Rel
Attach:[323] Enter Test Step ts_CMAC_Rel( 3 )
| 00:03:44.150 - Primitive: CMAC_Config_REQ Send event:[1] CMAC ! CMAC_Config_REQ = PDU (view PDU) 00:03:44.180 - Primitive: CMAC_Config_CNF begin "ca_CMAC_CfgCnf" of type CMAC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 8 against 8 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_CfgCnf" of type CMAC_Config_CNF Receive event:[2] CMAC ? CMAC_Config_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 8 ]} Attach:[323] Exit Test Step ts_CMAC_Rel
Attach:[324] Enter Test Step ts_CPHY_TrChRelNonDch( 3 )
| 00:03:44.180 - Primitive: CPHY_TrCH_Release_REQ Send event:[1] CPHY ! CPHY_TrCH_Release_REQ = PDU (view PDU) 00:03:44.200 - Primitive: CPHY_TrCH_Release_CNF begin "ca_PHY_RelCnf" of type CPHY_TrCH_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 8 against 8 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_PHY_RelCnf" of type CPHY_TrCH_Release_CNF Receive event:[2] CPHY ? CPHY_TrCH_Release_CNF = PDU (view PDU) Attach:[324] Exit Test Step ts_CPHY_TrChRelNonDch
Attach:[325] Enter Test Step ts_SS_StopRL( 3 )
| 00:03:44.200 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 7 ]} 00:03:44.210 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 7 against 7 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 7 ]} Attach:[325] Exit Test Step ts_SS_StopRL
Attach:[326] Enter Test Step ts_SS_StopRL( 3 )
| 00:03:44.210 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 8 ]} 00:03:44.230 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 8 against 8 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 8 ]} Attach:[326] Exit Test Step ts_SS_StopRL
Attach:[327] Enter Test Step ts_CRLC_Rel( 3 )
| 00:03:44.230 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:03:44.240 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -2 against -2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -2 ]} Attach:[327] Exit Test Step ts_CRLC_Rel
Attach:[328] Enter Test Step ts_CMAC_Rel( 3 )
| 00:03:44.240 - Primitive: CMAC_Config_REQ Send event:[1] CMAC ! CMAC_Config_REQ = PDU (view PDU) 00:03:44.260 - Primitive: CMAC_Config_CNF begin "ca_CMAC_CfgCnf" of type CMAC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 5 against 5 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_CfgCnf" of type CMAC_Config_CNF Receive event:[2] CMAC ? CMAC_Config_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 5 ]} Attach:[328] Exit Test Step ts_CMAC_Rel
Attach:[329] Enter Test Step ts_CPHY_TrChRelNonDch( 3 )
| 00:03:44.260 - Primitive: CPHY_TrCH_Release_REQ Send event:[1] CPHY ! CPHY_TrCH_Release_REQ = PDU (view PDU) 00:03:44.280 - Primitive: CPHY_TrCH_Release_CNF begin "ca_PHY_RelCnf" of type CPHY_TrCH_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 5 against 5 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_PHY_RelCnf" of type CPHY_TrCH_Release_CNF Receive event:[2] CPHY ? CPHY_TrCH_Release_CNF = PDU (view PDU) Attach:[329] Exit Test Step ts_CPHY_TrChRelNonDch
Attach:[330] Enter Test Step ts_SS_StopRL( 3 )
| 00:03:44.280 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 6 ]} 00:03:44.290 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 6 ]} Attach:[330] Exit Test Step ts_SS_StopRL
Attach:[331] Enter Test Step ts_SS_StopRL( 3 )
| 00:03:44.290 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 5 ]} 00:03:44.310 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 5 against 5 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 5 ]} Attach:[331] Exit Test Step ts_SS_StopRL
Attach:[4] Exit Test Step ts_SS_Rel::lt_ReleaseCommonCh
Attach:[5] Enter Test Step ts_SS_Rel::lt_Release_BCCH( 3 )
| Attach:[315] Enter Test Step ts_CRLC_Rel( 3 )
| 00:03:44.310 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:03:44.320 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} Attach:[315] Exit Test Step ts_CRLC_Rel
Attach:[316] Enter Test Step ts_CMAC_Rel( 3 )
| 00:03:44.320 - Primitive: CMAC_Config_REQ Send event:[1] CMAC ! CMAC_Config_REQ = PDU (view PDU) 00:03:44.340 - Primitive: CMAC_Config_CNF begin "ca_CMAC_CfgCnf" of type CMAC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_CfgCnf" of type CMAC_Config_CNF Receive event:[2] CMAC ? CMAC_Config_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 4 ]} Attach:[316] Exit Test Step ts_CMAC_Rel
Attach:[317] Enter Test Step ts_CPHY_TrChRelNonDch( 3 )
| 00:03:44.340 - Primitive: CPHY_TrCH_Release_REQ Send event:[1] CPHY ! CPHY_TrCH_Release_REQ = PDU (view PDU) 00:03:44.350 - Primitive: CPHY_TrCH_Release_CNF begin "ca_PHY_RelCnf" of type CPHY_TrCH_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_PHY_RelCnf" of type CPHY_TrCH_Release_CNF Receive event:[2] CPHY ? CPHY_TrCH_Release_CNF = PDU (view PDU) Attach:[317] Exit Test Step ts_CPHY_TrChRelNonDch
Attach:[318] Enter Test Step ts_SS_StopRL( 3 )
| 00:03:44.350 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 2 ]} 00:03:44.370 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 2 ]} Attach:[318] Exit Test Step ts_SS_StopRL
Attach:[319] Enter Test Step ts_SS_StopRL( 3 )
| 00:03:44.370 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 1 ]} 00:03:44.380 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 1 ]} Attach:[319] Exit Test Step ts_SS_StopRL
Attach:[320] Enter Test Step ts_SS_StopRL( 3 )
| 00:03:44.380 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 4 ]} 00:03:44.400 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 4 ]} Attach:[320] Exit Test Step ts_SS_StopRL
Attach:[321] Enter Test Step ts_SS_StopRL( 3 )
| 00:03:44.400 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 0 ]} 00:03:44.420 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 0 ]} Attach:[321] Exit Test Step ts_SS_StopRL
Attach:[5] Exit Test Step ts_SS_Rel::lt_Release_BCCH
Attach:[6] Enter Test Step ts_SetCellCfg( 3 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 3 )
| Assignment:[8] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Assignment:[2] cellConfig := cell_NotConfigured Attach:[3] Enter Test Step ts_SaveCellInfo( 3 )
| Assignment:[8] tcv_CellInfoD := (view Assignment) Attach:[3] Exit Test Step ts_SaveCellInfo
Attach:[6] Exit Test Step ts_SetCellCfg
Attach:[4] Exit Test Step ts_SS_Rel
Attach:[11] Exit Test Step po_ConnectionAndSS_Rel
Attach:[4] Exit Test Step po_ConnectionAndSS_Rels::lt_ReleaseCell
Attach:[5] Enter Test Step po_ConnectionAndSS_Rels::lt_ReleaseCell( 4 )
| Attach:[9] Enter Test Step ts_SetTmpCellInfo( 4 )
| Assignment:[10] tcv_TmpCellInfo := (view Assignment) Attach:[9] Exit Test Step ts_SetTmpCellInfo
Attach:[5] Exit Test Step po_ConnectionAndSS_Rels::lt_ReleaseCell
Attach:[6] Enter Test Step po_ConnectionAndSS_Rels::lt_ReleaseCell( 5 )
| Attach:[9] Enter Test Step ts_SetTmpCellInfo( 5 )
| Assignment:[12] tcv_TmpCellInfo := (view Assignment) Attach:[9] Exit Test Step ts_SetTmpCellInfo
Attach:[6] Exit Test Step po_ConnectionAndSS_Rels::lt_ReleaseCell
Attach:[7] Enter Test Step po_ConnectionAndSS_Rels::lt_ReleaseCell( 6 )
| Attach:[9] Enter Test Step ts_SetTmpCellInfo( 6 )
| Assignment:[14] tcv_TmpCellInfo := (view Assignment) Attach:[9] Exit Test Step ts_SetTmpCellInfo
Attach:[7] Exit Test Step po_ConnectionAndSS_Rels::lt_ReleaseCell
Attach:[8] Enter Test Step po_ConnectionAndSS_Rels::lt_ReleaseCell( 7 )
| Attach:[9] Enter Test Step ts_SetTmpCellInfo( 7 )
| Assignment:[16] tcv_TmpCellInfo := (view Assignment) Attach:[9] Exit Test Step ts_SetTmpCellInfo
Attach:[8] Exit Test Step po_ConnectionAndSS_Rels::lt_ReleaseCell
Attach:[11] Exit Test Step po_ConnectionAndSS_Rels
CancelTimer:[(implicit)] t_Guard [300] 300 s