| NAS_wk34-tc_12_4_1_2ps_2004-09-13_17.39.19

TTCN PDU: MMI_CmdReq

(To search, click here and then press Ctrl+F)

    {
      cmd: "Please set UE in operation mode A (to support simulataneous CS and PS services) "
    }

TTCN PDU: CPHY_Cell_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      tcell: 0,
      sfnOffset: 0,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      primaryScramblingCode_SS: 100,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      dLTxAttenuationLevel: 0
    }

TTCN PDU: CPHY_RL_Setup_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 0
      ],
      ratType: fdd,
      setupMessage:
      {
        physicalChannelInfo:
        [
          primaryCPICHInfo:
          {
            dl_TxPower_PCPICH: -60,
            txdiversityIndicator: GcFALSE
          }
        ]
      }
    }

TTCN PDU: CPHY_RL_Setup_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 1
      ],
      ratType: fdd,
      setupMessage:
      {
        physicalChannelInfo:
        [
          primarySCHInfo:
          {
            tstdIndicator: GcFALSE,
            dl_TxPower: -5
          }
        ]
      }
    }

TTCN PDU: CPHY_RL_Setup_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 2
      ],
      ratType: fdd,
      setupMessage:
      {
        physicalChannelInfo:
        [
          secondarySCHInfo:
          {
            tstdIndicator: GcFALSE,
            dl_TxPower: -5
          }
        ]
      }
    }

TTCN PDU: CPHY_RL_Setup_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 4
      ],
      ratType: fdd,
      setupMessage:
      {
        physicalChannelInfo:
        [
          primaryCCPCHInfo:
          {
            sttd_Indicator: GcFALSE,
            dl_TxPower: -2
          }
        ]
      }
    }

TTCN PDU: CPHY_TrCH_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 4
      ],
      ratType: fdd,
      trchConfigType:
      [
        nonDch: NULL
      ],
      configMessage:
      {
        activationTime:
        [
          activateNow: NULL
        ],
        ulconnectedTrCHList: OMIT,
        ulTFCS: OMIT,
        dlconnectedTrCHList:
        [
          {
            trchid: 11,
            dl_TransportChannelType: bch,
            transportChannelInfo:
            {
              tti:
              [
                tti20:
                [
                  {
                    tb_Size: 246,
                    numberOfTbSizeList:
                    [
                      [
                        one: NULL
                      ]
                    ],
                    logicalChannelList:
                    [
                      configured: NULL
                    ]
                  }
                ]
              ],
              semistaticTF_Information:
              {
                channelCodingType:
                [
                  convolutional: half
                ],
                rateMatchingAttribute# 1 # crc_Size# crc16
              }
            }
          }
        ]
        # dlTFCS#
        [
          normalTFCI_Signalling#
          [
            complete#
            {
              ctfcSize#
              [
                ctfc2Bit#
                [
                  {
                    ctfc2# 0 # powerOffsetInformation#
                    {
                      gainFactorInformation#
                      [
                        signalledGainFactors#
                        {
                          modeSpecificInfo#
                          [
                            fdd#
                            {
                              gainFactorBetaC# 11
                            }
                          ]
                          # gainFactorBetaD# 15 # referenceTFC_ID# 0
                        }
                      ]
                      # powerOffsetPp_m# OMIT
                    }
                  }
                ]
              ]
            }
          ]
        ]
      }
    }

TTCN PDU: CPHY_TrCH_Config_CNF

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 4
      ]
    }

TTCN PDU: CMAC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 4
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          activationTime:
          [
            activateNow: NULL
          ],
          uE_Info:
          {
            u_RNTI: OMIT,
            c_RNTI: OMIT
          },
          trCHInfo:
          {
            ulconnectedTrCHList: OMIT,
            ulTFCS: OMIT,
            dlconnectedTrCHList:
            [
              {
                trchid: 11,
                transportChannelInfo:
                {
                  tti:
                  [
                    tti20:
                    [
                      {
                        tb_Size: 246,
                        numberOfTbSizeList:
                        [
                          [
                            one: NULL
                          ]
                        ],
                        logicalChannelList:
                        [
                          configured: NULL
                        ]
                      }
                    ]
                  ],
                  semistaticTF_Information:
                  {
                    channelCodingType:
                    [
                      convolutional: half
                    ],
                    rateMatchingAttribute# 1 # crc_Size# crc16
                  }
                }
              }
            ]
            # dlTFCS#
            [
              normalTFCI_Signalling#
              [
                complete#
                {
                  ctfcSize#
                  [
                    ctfc2Bit#
                    [
                      {
                        ctfc2# 0 # powerOffsetInformation#
                        {
                          gainFactorInformation#
                          [
                            signalledGainFactors#
                            {
                              modeSpecificInfo#
                              [
                                fdd#
                                {
                                  gainFactorBetaC# 11
                                }
                              ]
                              # gainFactorBetaD# 15 # referenceTFC_ID# 0
                            }
                          ]
                          # powerOffsetPp_m# OMIT
                        }
                      }
                    ]
                  ]
                }
              ]
            ]
          }
          # trCH_LogCHMapping#
          {
            ulconnectedTrCHList# OMIT# dlconnectedTrCHList#
            [
              {
                trchid# 11 # trCH_LogCHMappingList#
                [
                  {
                    logicalChannel_Mapping#
                    [
                      dl_LogicalChannelMapping#
                      {
                        macHeaderManipulation# normalMacHeader# dl_TransportChannelType# bch# logicalChannelIdentity# 1 # logicalChannelType# bCCH# rlc_SizeList#
                        [
                          configured# NULL
                        ]
                        # mac_LogicalChannelPriority# 1
                      }
                    ]
                    # rB_Identity# #1 # cn_DomainIdentity# OMIT
                  }
                ]
              }
            ]
          }
        }
      ]
    }

TTCN PDU: CPHY_RL_Setup_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 5
      ],
      ratType: fdd,
      setupMessage:
      {
        physicalChannelInfo:
        [
          secondaryCCPCHInfo:
          {
            scramblingCode: 0,
            dl_ChannelizationCode:
            [
              sf64: 1
            ],
            sCCPCHSlotFormat: 8,
            timingOffset: 0,
            positionFixedOrFlexible: flexible,
            sttd_Indicator: GcFALSE,
            dl_TxPower: -2,
            powerOffsetOfTFCI_PO1: 6,
            powerOffsetOfPILOT_PO3: 6
          }
        ]
      }
    }

TTCN PDU: CPHY_TrCH_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 5
      ],
      ratType: fdd,
      trchConfigType:
      [
        nonDch: NULL
      ],
      configMessage:
      {
        activationTime:
        [
          activateNow: NULL
        ],
        ulconnectedTrCHList: OMIT,
        ulTFCS: OMIT,
        dlconnectedTrCHList:
        [
          {
            trchid: 12,
            dl_TransportChannelType: pch,
            transportChannelInfo:
            {
              tti:
              [
                tti10:
                [
                  {
                    tb_Size: 240,
                    numberOfTbSizeList:
                    [
                      [
                        zero: NULL
                      ],

                      [
                        one: NULL
                      ]
                    ],
                    logicalChannelList:
                    [
                      allSizes: NULL
                    ]
                  }
                ]
              ],
              semistaticTF_Information:
              {
                channelCodingType:
                [
                  convolutional: half
                ],
                rateMatchingAttribute# 230 # crc_Size# crc16
              }
            }
          }
          #
          {
            trchid# 13 # dl_TransportChannelType# fach# transportChannelInfo#
            {
              tti#
              [
                tti10#
                [
                  {
                    tb_Size# 168 # numberOfTbSizeList#
                    [
                      [
                        zero# NULL
                      ]
                      #
                      [
                        one# NULL
                      ]
                      #
                      [
                        small# 2
                      ]
                    ]
                    # logicalChannelList#
                    [
                      allSizes# NULL
                    ]
                  }
                ]
              ]
              # semistaticTF_Information#
              {
                channelCodingType#
                [
                  convolutional# half
                ]
                # rateMatchingAttribute# 220 # crc_Size# crc16
              }
            }
          }
          #
          {
            trchid# 14 # dl_TransportChannelType# fach# transportChannelInfo#
            {
              tti#
              [
                tti10#
                [
                  {
                    tb_Size# 360 # numberOfTbSizeList#
                    [
                      [
                        zero# NULL
                      ]
                      #
                      [
                        one# NULL
                      ]
                    ]
                    # logicalChannelList#
                    [
                      allSizes# NULL
                    ]
                  }
                ]
              ]
              # semistaticTF_Information#
              {
                channelCodingType#
                [
                  turbo# NULL
                ]
                # rateMatchingAttribute# 130 # crc_Size# crc16
              }
            }
          }
        ]
        # dlTFCS#
        [
          normalTFCI_Signalling#
          [
            complete#
            {
              ctfcSize#
              [
                ctfc4Bit#
                [
                  {
                    ctfc4# 0 # powerOffsetInformation#
                    {
                      gainFactorInformation#
                      [
                        computedGainFactors# 0
                      ]
                      # powerOffsetPp_m# OMIT
                    }
                  }
                  #
                  {
                    ctfc4# 1 # powerOffsetInformation#
                    {
                      gainFactorInformation#
                      [
                        computedGainFactors# 0
                      ]
                      # powerOffsetPp_m# OMIT
                    }
                  }
                  #
                  {
                    ctfc4# 2 # powerOffsetInformation#
                    {
                      gainFactorInformation#
                      [
                        computedGainFactors# 0
                      ]
                      # powerOffsetPp_m# OMIT
                    }
                  }
                  #
                  {
                    ctfc4# 3 # powerOffsetInformation#
                    {
                      gainFactorInformation#
                      [
                        computedGainFactors# 0
                      ]
                      # powerOffsetPp_m# OMIT
                    }
                  }
                  #
                  {
                    ctfc4# 4 # powerOffsetInformation#
                    {
                      gainFactorInformation#
                      [
                        computedGainFactors# 0
                      ]
                      # powerOffsetPp_m# OMIT
                    }
                  }
                  #
                  {
                    ctfc4# 5 # powerOffsetInformation#
                    {
                      gainFactorInformation#
                      [
                        computedGainFactors# 0
                      ]
                      # powerOffsetPp_m# OMIT
                    }
                  }
                  #
                  {
                    ctfc4# 6 # powerOffsetInformation#
                    {
                      gainFactorInformation#
                      [
                        computedGainFactors# 0
                      ]
                      # powerOffsetPp_m# OMIT
                    }
                  }
                  #
                  {
                    ctfc4# 8 # powerOffsetInformation#
                    {
                      gainFactorInformation#
                      [
                        signalledGainFactors#
                        {
                          modeSpecificInfo#
                          [
                            fdd#
                            {
                              gainFactorBetaC# 11
                            }
                          ]
                          # gainFactorBetaD# 15 # referenceTFC_ID# 0
                        }
                      ]
                      # powerOffsetPp_m# OMIT
                    }
                  }
                ]
              ]
            }
          ]
        ]
      }
    }

TTCN PDU: CMAC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 5
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          activationTime:
          [
            activateNow: NULL
          ],
          uE_Info:
          {
            u_RNTI: OMIT,
            c_RNTI: OMIT
          },
          trCHInfo:
          {
            ulconnectedTrCHList: OMIT,
            ulTFCS: OMIT,
            dlconnectedTrCHList:
            [
              {
                trchid: 12,
                transportChannelInfo:
                {
                  tti:
                  [
                    tti10:
                    [
                      {
                        tb_Size: 240,
                        numberOfTbSizeList:
                        [
                          [
                            zero: NULL
                          ],

                          [
                            one: NULL
                          ]
                        ],
                        logicalChannelList:
                        [
                          allSizes: NULL
                        ]
                      }
                    ]
                  ],
                  semistaticTF_Information:
                  {
                    channelCodingType:
                    [
                      convolutional: half
                    ],
                    rateMatchingAttribute# 230 # crc_Size# crc16
                  }
                }
              }
              #
              {
                trchid# 13 # transportChannelInfo#
                {
                  tti#
                  [
                    tti10#
                    [
                      {
                        tb_Size# 168 # numberOfTbSizeList#
                        [
                          [
                            zero# NULL
                          ]
                          #
                          [
                            one# NULL
                          ]
                          #
                          [
                            small# 2
                          ]
                        ]
                        # logicalChannelList#
                        [
                          allSizes# NULL
                        ]
                      }
                    ]
                  ]
                  # semistaticTF_Information#
                  {
                    channelCodingType#
                    [
                      convolutional# half
                    ]
                    # rateMatchingAttribute# 220 # crc_Size# crc16
                  }
                }
              }
              #
              {
                trchid# 14 # transportChannelInfo#
                {
                  tti#
                  [
                    tti10#
                    [
                      {
                        tb_Size# 360 # numberOfTbSizeList#
                        [
                          [
                            zero# NULL
                          ]
                          #
                          [
                            one# NULL
                          ]
                        ]
                        # logicalChannelList#
                        [
                          allSizes# NULL
                        ]
                      }
                    ]
                  ]
                  # semistaticTF_Information#
                  {
                    channelCodingType#
                    [
                      turbo# NULL
                    ]
                    # rateMatchingAttribute# 130 # crc_Size# crc16
                  }
                }
              }
            ]
            # dlTFCS#
            [
              normalTFCI_Signalling#
              [
                complete#
                {
                  ctfcSize#
                  [
                    ctfc4Bit#
                    [
                      {
                        ctfc4# 0 # powerOffsetInformation#
                        {
                          gainFactorInformation#
                          [
                            computedGainFactors# 0
                          ]
                          # powerOffsetPp_m# OMIT
                        }
                      }
                      #
                      {
                        ctfc4# 1 # powerOffsetInformation#
                        {
                          gainFactorInformation#
                          [
                            computedGainFactors# 0
                          ]
                          # powerOffsetPp_m# OMIT
                        }
                      }
                      #
                      {
                        ctfc4# 2 # powerOffsetInformation#
                        {
                          gainFactorInformation#
                          [
                            computedGainFactors# 0
                          ]
                          # powerOffsetPp_m# OMIT
                        }
                      }
                      #
                      {
                        ctfc4# 3 # powerOffsetInformation#
                        {
                          gainFactorInformation#
                          [
                            computedGainFactors# 0
                          ]
                          # powerOffsetPp_m# OMIT
                        }
                      }
                      #
                      {
                        ctfc4# 4 # powerOffsetInformation#
                        {
                          gainFactorInformation#
                          [
                            computedGainFactors# 0
                          ]
                          # powerOffsetPp_m# OMIT
                        }
                      }
                      #
                      {
                        ctfc4# 5 # powerOffsetInformation#
                        {
                          gainFactorInformation#
                          [
                            computedGainFactors# 0
                          ]
                          # powerOffsetPp_m# OMIT
                        }
                      }
                      #
                      {
                        ctfc4# 6 # powerOffsetInformation#
                        {
                          gainFactorInformation#
                          [
                            computedGainFactors# 0
                          ]
                          # powerOffsetPp_m# OMIT
                        }
                      }
                      #
                      {
                        ctfc4# 8 # powerOffsetInformation#
                        {
                          gainFactorInformation#
                          [
                            signalledGainFactors#
                            {
                              modeSpecificInfo#
                              [
                                fdd#
                                {
                                  gainFactorBetaC# 11
                                }
                              ]
                              # gainFactorBetaD# 15 # referenceTFC_ID# 0
                            }
                          ]
                          # powerOffsetPp_m# OMIT
                        }
                      }
                    ]
                  ]
                }
              ]
            ]
          }
          # trCH_LogCHMapping#
          {
            ulconnectedTrCHList# OMIT# dlconnectedTrCHList#
            [
              {
                trchid# 12 # trCH_LogCHMappingList#
                [
                  {
                    logicalChannel_Mapping#
                    [
                      dl_LogicalChannelMapping#
                      {
                        macHeaderManipulation# normalMacHeader# dl_TransportChannelType# pch# logicalChannelIdentity# 1 # logicalChannelType# pCCH# rlc_SizeList#
                        [
                          configured# NULL
                        ]
                        # mac_LogicalChannelPriority# 1
                      }
                    ]
                    # rB_Identity# #2 # cn_DomainIdentity# OMIT
                  }
                ]
              }
              #
              {
                trchid# 13 # trCH_LogCHMappingList#
                [
                  {
                    logicalChannel_Mapping#
                    [
                      dl_LogicalChannelMapping#
                      {
                        macHeaderManipulation# normalMacHeader# dl_TransportChannelType# fach# logicalChannelIdentity# 5 # logicalChannelType# cCCH# rlc_SizeList#
                        [
                          configured# NULL
                        ]
                        # mac_LogicalChannelPriority# 1
                      }
                    ]
                    # rB_Identity# 0 # cn_DomainIdentity# OMIT
                  }
                ]
              }
            ]
          }
        }
      ]
    }

TTCN PDU: CPHY_RL_Setup_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 6
      ],
      ratType: fdd,
      setupMessage:
      {
        physicalChannelInfo:
        [
          pICHInfo:
          {
            pichinfo:
            [
              fdd:
              {
                channelisationCode256: 2,
                pi_CountPerFrame: e18,
                sttd_Indicator: GcFALSE
              }
            ],
            dl_TxPower: -5,
            sccpchId_associated: 5
          }
        ]
      }
    }

TTCN PDU: CPHY_RL_Setup_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 7
      ],
      ratType: fdd,
      setupMessage:
      {
        physicalChannelInfo:
        [
          aICHInfo:
          {
            aichinfo:
            {
              channelisationCode256: 3,
              sttd_Indicator: GcFALSE,
              aich_TransmissionTiming: e0
            },
            dl_TxPower: -5
          }
        ]
      }
    }

TTCN PDU: CPHY_RL_Setup_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 8
      ],
      ratType: fdd,
      setupMessage:
      {
        physicalChannelInfo:
        [
          pRACHInfo:
          {
            fdd_tdd:
            [
              fdd:
              {
                preambleSignature: '0000000011111111'B,
                spreadingFactorForDataPart: sfpr64,
                preambleScramblingCode: 0,
                puncturingLimit: pl1,
                accessSlot: '111111111111'B
              }
            ]
          }
        ]
      }
    }

TTCN PDU: CPHY_TrCH_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 8
      ],
      ratType: fdd,
      trchConfigType:
      [
        nonDch: NULL
      ],
      configMessage:
      {
        activationTime:
        [
          activateNow: NULL
        ],
        ulconnectedTrCHList:
        [
          {
            trchid: 15,
            ul_TransportChannelType: rach,
            transportChannelInfo:
            {
              tti:
              [
                tti20:
                [
                  {
                    tb_Size: 168,
                    numberOfTbSizeList:
                    [
                      [
                        one: NULL
                      ]
                    ],
                    logicalChannelList:
                    [
                      configured: NULL
                    ]
                  },

                  {
                    tb_Size: 360,
                    numberOfTbSizeList:
                    [
                      [
                        one: NULL
                      ]
                    ],
                    logicalChannelList:
                    [
                      configured: NULL
                    ]
                  }
                ]
              ],
              semistaticTF_Information:
              {
                channelCodingType:
                [
                  convolutional: half
                ],
                rateMatchingAttribute# 150 # crc_Size# crc16
              }
            }
          }
        ]
        # ulTFCS#
        [
          normalTFCI_Signalling#
          [
            complete#
            {
              ctfcSize#
              [
                ctfc2Bit#
                [
                  {
                    ctfc2# 0 # powerOffsetInformation# OMIT
                  }
                  #
                  {
                    ctfc2# 1 # powerOffsetInformation# OMIT
                  }
                ]
              ]
            }
          ]
        ]
        # dlconnectedTrCHList# OMIT# dlTFCS# OMIT
      }
    }

TTCN PDU: CMAC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 8
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          activationTime:
          [
            activateNow: NULL
          ],
          uE_Info:
          {
            u_RNTI: OMIT,
            c_RNTI: OMIT
          },
          trCHInfo:
          {
            ulconnectedTrCHList:
            [
              {
                trchid: 15,
                transportChannelInfo:
                {
                  tti:
                  [
                    tti20:
                    [
                      {
                        tb_Size: 168,
                        numberOfTbSizeList:
                        [
                          [
                            one: NULL
                          ]
                        ],
                        logicalChannelList:
                        [
                          configured: NULL
                        ]
                      },

                      {
                        tb_Size: 360,
                        numberOfTbSizeList:
                        [
                          [
                            one: NULL
                          ]
                        ],
                        logicalChannelList:
                        [
                          configured: NULL
                        ]
                      }
                    ]
                  ],
                  semistaticTF_Information:
                  {
                    channelCodingType:
                    [
                      convolutional: half
                    ],
                    rateMatchingAttribute# 150 # crc_Size# crc16
                  }
                }
              }
            ]
            # ulTFCS#
            [
              normalTFCI_Signalling#
              [
                complete#
                {
                  ctfcSize#
                  [
                    ctfc2Bit#
                    [
                      {
                        ctfc2# 0 # powerOffsetInformation# OMIT
                      }
                      #
                      {
                        ctfc2# 1 # powerOffsetInformation# OMIT
                      }
                    ]
                  ]
                }
              ]
            ]
            # dlconnectedTrCHList# OMIT# dlTFCS# OMIT
          }
          # trCH_LogCHMapping#
          {
            ulconnectedTrCHList#
            [
              {
                trchid# 15 # trCH_LogCHMappingList#
                [
                  {
                    logicalChannel_Mapping#
                    [
                      ul_LogicalChannelMapping#
                      {
                        macHeaderManipulation# normalMacHeader# ul_TransportChannelType# rach# logicalChannelIdentity# 5 # logicalChannelType# cCCH
                      }
                    ]
                    # rB_Identity# 0 # cn_DomainIdentity# OMIT
                  }
                ]
              }
            ]
            # dlconnectedTrCHList# OMIT
          }
        }
      ]
    }

TTCN PDU: CPHY_RL_Setup_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 26
      ],
      ratType: fdd,
      setupMessage:
      {
        physicalChannelInfo:
        [
          dPCHInfo:
          {
            ul_DPCHInfo: OMIT,
            dl_DPCHInfo:
            {
              dl_CommonInformation:
              {
                dl_DPCH_InfoCommon:
                {
                  cfnHandling:
                  [
                    initialise:
                    {
                      cfntargetsfnframeoffset: OMIT
                    }
                  ],
                  modeSpecificInfo:
                  [
                    fdd:
                    {
                      dl_DPCH_PowerControlInfo:
                      {
                        modeSpecificInfo:
                        [
                          fdd:
                          {
                            dpc_Mode: singleTPC
                          }
                        ]
                      },
                      powerOffsetPilot_pdpdch: 0,
                      dl_rate_matching_restriction: OMIT,
                      spreadingFactorAndPilot:
                      [
                        sfd128: pb4
                      ],
                      positionFixedOrFlexible: fixed,
                      tfci_Existence: GcFALSE
                    }
                  ]
                },
                modeSpecificInfo:
                [
                  fdd:
                  {
                    defaultDPCH_OffsetValue: 0,
                    dpch_CompressedModeInfo: OMIT,
                    tx_DiversityMode: noDiversity,
                    ssdt_Information: OMIT
                  }
                ]
              },
              dl_DPCH_InfoPerRL:
              [
                fdd:
                {
                  pCPICH_UsageForChannelEst: mayBeUsed,
                  dpch_FrameOffset: 0,
                  secondaryCPICH_Info: OMIT,
                  dl_ChannelisationCodeList:
                  [
                    {
                      secondaryScramblingCode: 1,
                      sf_AndCodeNumber:
                      [
                        sf128: 0
                      ],
                      scramblingCodeChange: OMIT
                    }
                  ],
                  tpc_CombinationIndex: 0,
                  ssdt_CellIdentity: OMIT,
                  closedLoopTimingAdjMode: OMIT
                }
              ],
              powerOffsetOfTFCI_PO1: 0,
              powerOffsetOfTPC_PO2: 0,
              powerOffsetOfPILOT_PO3: 0,
              dl_TxPower: -5,
              dl_TxPowerMax: 15,
              dl_TxPowerMin: -35
            }
          }
        ]
      }
    }

TTCN PDU: CPHY_TrCH_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 26
      ],
      ratType: fdd,
      trchConfigType:
      [
        dch: normal
      ],
      configMessage:
      {
        activationTime:
        [
          activateNow: NULL
        ],
        ulconnectedTrCHList: OMIT,
        ulTFCS: OMIT,
        dlconnectedTrCHList:
        [
          {
            trchid: 10,
            dl_TransportChannelType: dch,
            transportChannelInfo:
            {
              tti:
              [
                tti10:
                [
                  {
                    tb_Size: 148,
                    numberOfTbSizeList:
                    [
                      [
                        zero: NULL
                      ],

                      [
                        one: NULL
                      ]
                    ],
                    logicalChannelList:
                    [
                      allSizes: NULL
                    ]
                  }
                ]
              ],
              semistaticTF_Information:
              {
                channelCodingType:
                [
                  convolutional: third
                ],
                rateMatchingAttribute# 192 # crc_Size# crc16
              }
            }
          }
        ]
        # dlTFCS#
        [
          normalTFCI_Signalling#
          [
            complete#
            {
              ctfcSize#
              [
                ctfc2Bit#
                [
                  {
                    ctfc2# 0 # powerOffsetInformation#
                    {
                      gainFactorInformation#
                      [
                        computedGainFactors# 0
                      ]
                      # powerOffsetPp_m# OMIT
                    }
                  }
                  #
                  {
                    ctfc2# 1 # powerOffsetInformation#
                    {
                      gainFactorInformation#
                      [
                        signalledGainFactors#
                        {
                          modeSpecificInfo#
                          [
                            fdd#
                            {
                              gainFactorBetaC# 11
                            }
                          ]
                          # gainFactorBetaD# 15 # referenceTFC_ID# 0
                        }
                      ]
                      # powerOffsetPp_m# OMIT
                    }
                  }
                ]
              ]
            }
          ]
        ]
      }
    }

TTCN PDU: CPHY_TrCH_Config_CNF

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 26
      ]
    }

TTCN PDU: CMAC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        physicalChannelIdentity: 26
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          activationTime:
          [
            activateNow: NULL
          ],
          uE_Info:
          {
            u_RNTI: OMIT,
            c_RNTI: OMIT
          },
          trCHInfo:
          {
            ulconnectedTrCHList: OMIT,
            ulTFCS: OMIT,
            dlconnectedTrCHList:
            [
              {
                trchid: 10,
                transportChannelInfo:
                {
                  tti:
                  [
                    tti10:
                    [
                      {
                        tb_Size: 148,
                        numberOfTbSizeList:
                        [
                          [
                            zero: NULL
                          ],

                          [
                            one: NULL
                          ]
                        ],
                        logicalChannelList:
                        [
                          allSizes: NULL
                        ]
                      }
                    ]
                  ],
                  semistaticTF_Information:
                  {
                    channelCodingType:
                    [
                      convolutional: third
                    ],
                    rateMatchingAttribute# 192 # crc_Size# crc16
                  }
                }
              }
            ]
            # dlTFCS#
            [
              normalTFCI_Signalling#
              [
                complete#
                {
                  ctfcSize#
                  [
                    ctfc2Bit#
                    [
                      {
                        ctfc2# 0 # powerOffsetInformation#
                        {
                          gainFactorInformation#
                          [
                            computedGainFactors# 0
                          ]
                          # powerOffsetPp_m# OMIT
                        }
                      }
                      #
                      {
                        ctfc2# 1 # powerOffsetInformation#
                        {
                          gainFactorInformation#
                          [
                            signalledGainFactors#
                            {
                              modeSpecificInfo#
                              [
                                fdd#
                                {
                                  gainFactorBetaC# 11
                                }
                              ]
                              # gainFactorBetaD# 15 # referenceTFC_ID# 0
                            }
                          ]
                          # powerOffsetPp_m# OMIT
                        }
                      }
                    ]
                  ]
                }
              ]
            ]
          }
          # trCH_LogCHMapping#
          {
            ulconnectedTrCHList# OMIT# dlconnectedTrCHList#
            [
              {
                trchid# 10 # trCH_LogCHMappingList#
                [
                  {
                    logicalChannel_Mapping#
                    [
                      dl_LogicalChannelMapping#
                      {
                        macHeaderManipulation# normalMacHeader# dl_TransportChannelType# dch# logicalChannelIdentity# 1 # logicalChannelType# dCCH# rlc_SizeList#
                        [
                          configured# NULL
                        ]
                        # mac_LogicalChannelPriority# 1
                      }
                    ]
                    # rB_Identity# 1 # cn_DomainIdentity# OMIT
                  }
                  #
                  {
                    logicalChannel_Mapping#
                    [
                      dl_LogicalChannelMapping#
                      {
                        macHeaderManipulation# normalMacHeader# dl_TransportChannelType# dch# logicalChannelIdentity# 2 # logicalChannelType# dCCH# rlc_SizeList#
                        [
                          configured# NULL
                        ]
                        # mac_LogicalChannelPriority# 2
                      }
                    ]
                    # rB_Identity# 2 # cn_DomainIdentity# OMIT
                  }
                  #
                  {
                    logicalChannel_Mapping#
                    [
                      dl_LogicalChannelMapping#
                      {
                        macHeaderManipulation# normalMacHeader# dl_TransportChannelType# dch# logicalChannelIdentity# 3 # logicalChannelType# dCCH# rlc_SizeList#
                        [
                          configured# NULL
                        ]
                        # mac_LogicalChannelPriority# 3
                      }
                    ]
                    # rB_Identity# 3 # cn_DomainIdentity# OMIT
                  }
                  #
                  {
                    logicalChannel_Mapping#
                    [
                      dl_LogicalChannelMapping#
                      {
                        macHeaderManipulation# normalMacHeader# dl_TransportChannelType# dch# logicalChannelIdentity# 4 # logicalChannelType# dCCH# rlc_SizeList#
                        [
                          configured# NULL
                        ]
                        # mac_LogicalChannelPriority# 4
                      }
                    ]
                    # rB_Identity# 4 # cn_DomainIdentity# OMIT
                  }
                ]
              }
            ]
          }
        }
      ]
    }

TTCN PDU: CPHY_RL_Setup_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 20
      ],
      ratType: fdd,
      setupMessage:
      {
        physicalChannelInfo:
        [
          dPCHInfo:
          {
            ul_DPCHInfo:
            {
              ul_DPCH_PowerControlInfo:
              [
                fdd:
                {
                  dpcch_PowerOffset: -40,
                  pc_Preamble: 1,
                  sRB_delay: 7,
                  powerControlAlgorithm:
                  [
                    algorithm1: 0
                  ]
                }
              ],
              modeSpecificInfo:
              [
                fdd:
                {
                  scramblingCodeType: longSC,
                  scramblingCode: 0,
                  numberOfDPDCH: OMIT,
                  spreadingFactor: sf64,
                  tfci_Existence: GcTRUE,
                  numberOfFBI_Bits: OMIT,
                  puncturingLimit: pl1
                }
              ]
            },
            dl_DPCHInfo: OMIT
          }
        ]
      }
    }

TTCN PDU: CPHY_TrCH_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 20
      ],
      ratType: fdd,
      trchConfigType:
      [
        dch: normal
      ],
      configMessage:
      {
        activationTime:
        [
          activateNow: NULL
        ],
        ulconnectedTrCHList:
        [
          {
            trchid: 5,
            ul_TransportChannelType: dch,
            transportChannelInfo:
            {
              tti:
              [
                tti10:
                [
                  {
                    tb_Size: 148,
                    numberOfTbSizeList:
                    [
                      [
                        zero: NULL
                      ],

                      [
                        one: NULL
                      ]
                    ],
                    logicalChannelList:
                    [
                      allSizes: NULL
                    ]
                  }
                ]
              ],
              semistaticTF_Information:
              {
                channelCodingType:
                [
                  convolutional: third
                ],
                rateMatchingAttribute# 192 # crc_Size# crc16
              }
            }
          }
        ]
        # ulTFCS#
        [
          normalTFCI_Signalling#
          [
            complete#
            {
              ctfcSize#
              [
                ctfc2Bit#
                [
                  {
                    ctfc2# 0 # powerOffsetInformation# OMIT
                  }
                  #
                  {
                    ctfc2# 1 # powerOffsetInformation# OMIT
                  }
                ]
              ]
            }
          ]
        ]
        # dlconnectedTrCHList# OMIT# dlTFCS# OMIT
      }
    }

TTCN PDU: CPHY_TrCH_Config_CNF

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 20
      ]
    }

TTCN PDU: CMAC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        physicalChannelIdentity: 20
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          activationTime:
          [
            activateNow: NULL
          ],
          uE_Info:
          {
            u_RNTI: OMIT,
            c_RNTI: OMIT
          },
          trCHInfo:
          {
            ulconnectedTrCHList:
            [
              {
                trchid: 5,
                transportChannelInfo:
                {
                  tti:
                  [
                    tti10:
                    [
                      {
                        tb_Size: 148,
                        numberOfTbSizeList:
                        [
                          [
                            zero: NULL
                          ],

                          [
                            one: NULL
                          ]
                        ],
                        logicalChannelList:
                        [
                          allSizes: NULL
                        ]
                      }
                    ]
                  ],
                  semistaticTF_Information:
                  {
                    channelCodingType:
                    [
                      convolutional: third
                    ],
                    rateMatchingAttribute# 192 # crc_Size# crc16
                  }
                }
              }
            ]
            # ulTFCS#
            [
              normalTFCI_Signalling#
              [
                complete#
                {
                  ctfcSize#
                  [
                    ctfc2Bit#
                    [
                      {
                        ctfc2# 0 # powerOffsetInformation# OMIT
                      }
                      #
                      {
                        ctfc2# 1 # powerOffsetInformation# OMIT
                      }
                    ]
                  ]
                }
              ]
            ]
            # dlconnectedTrCHList# OMIT# dlTFCS# OMIT
          }
          # trCH_LogCHMapping#
          {
            ulconnectedTrCHList#
            [
              {
                trchid# 5 # trCH_LogCHMappingList#
                [
                  {
                    logicalChannel_Mapping#
                    [
                      ul_LogicalChannelMapping#
                      {
                        macHeaderManipulation# normalMacHeader# ul_TransportChannelType# dch# logicalChannelIdentity# 1 # logicalChannelType# dCCH
                      }
                    ]
                    # rB_Identity# 1 # cn_DomainIdentity# OMIT
                  }
                  #
                  {
                    logicalChannel_Mapping#
                    [
                      ul_LogicalChannelMapping#
                      {
                        macHeaderManipulation# normalMacHeader# ul_TransportChannelType# dch# logicalChannelIdentity# 2 # logicalChannelType# dCCH
                      }
                    ]
                    # rB_Identity# 2 # cn_DomainIdentity# OMIT
                  }
                  #
                  {
                    logicalChannel_Mapping#
                    [
                      ul_LogicalChannelMapping#
                      {
                        macHeaderManipulation# normalMacHeader# ul_TransportChannelType# dch# logicalChannelIdentity# 3 # logicalChannelType# dCCH
                      }
                    ]
                    # rB_Identity# 3 # cn_DomainIdentity# OMIT
                  }
                  #
                  {
                    logicalChannel_Mapping#
                    [
                      ul_LogicalChannelMapping#
                      {
                        macHeaderManipulation# normalMacHeader# ul_TransportChannelType# dch# logicalChannelIdentity# 4 # logicalChannelType# dCCH
                      }
                    ]
                    # rB_Identity# 4 # cn_DomainIdentity# OMIT
                  }
                ]
              }
            ]
            # dlconnectedTrCHList# OMIT
          }
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          sS_rlc_Info:
          {
            sS_ul_RLC_Mode: OMIT,
            sS_dl_RLC_Mode:
            {
              dl_PayloadSize: 246,
              dl_RLCModeInfo:
              [
                ul_TM_RLC_Mode:
                {
                  transmissionRLC_Discard: OMIT,
                  segmentationIndication: GcFALSE
                }
              ]
            }
          },
          rB_LogCH_Mapping:
          {
            uLlogicalChannelIdentity: OMIT,
            dLlogicalChannelIdentity: 1,
            logicalChannelType: OMIT,
            cn_DomainIdentity: OMIT
          }
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -2
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          sS_rlc_Info:
          {
            sS_ul_RLC_Mode: OMIT,
            sS_dl_RLC_Mode:
            {
              dl_PayloadSize: 240,
              dl_RLCModeInfo:
              [
                ul_TM_RLC_Mode:
                {
                  transmissionRLC_Discard: OMIT,
                  segmentationIndication: GcFALSE
                }
              ]
            }
          },
          rB_LogCH_Mapping:
          {
            uLlogicalChannelIdentity: OMIT,
            dLlogicalChannelIdentity: 1,
            logicalChannelType: OMIT,
            cn_DomainIdentity: OMIT
          }
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: 0
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          sS_rlc_Info:
          {
            sS_ul_RLC_Mode: OMIT,
            sS_dl_RLC_Mode:
            {
              dl_PayloadSize: 152,
              dl_RLCModeInfo:
              [
                ul_UM_RLC_Mode:
                {
                  transmissionRLC_Discard:
                  [
                    timerBasedNoExplicit: dt100
                  ]
                }
              ]
            }
          },
          rB_LogCH_Mapping:
          {
            uLlogicalChannelIdentity: OMIT,
            dLlogicalChannelIdentity: 5,
            logicalChannelType: OMIT,
            cn_DomainIdentity: OMIT
          }
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: 0
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          sS_rlc_Info:
          {
            sS_ul_RLC_Mode:
            [
              dl_TM_RLC_Mode:
              {
                segmentationIndication: GcFALSE
              }
            ],
            sS_dl_RLC_Mode:
            {
              dl_PayloadSize: 166,
              dl_RLCModeInfo:
              [
                ul_TM_RLC_Mode:
                {
                  transmissionRLC_Discard: OMIT,
                  segmentationIndication: GcFALSE
                }
              ]
            }
          },
          rB_LogCH_Mapping:
          {
            uLlogicalChannelIdentity: 5,
            dLlogicalChannelIdentity: OMIT,
            logicalChannelType: OMIT,
            cn_DomainIdentity: OMIT
          }
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 1
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          sS_rlc_Info:
          {
            sS_ul_RLC_Mode:
            [
              dl_UM_RLC_Mode: NULL
            ],
            sS_dl_RLC_Mode:
            {
              dl_PayloadSize: 136,
              dl_RLCModeInfo:
              [
                ul_UM_RLC_Mode:
                {
                  transmissionRLC_Discard:
                  [
                    timerBasedNoExplicit: dt100
                  ]
                }
              ]
            }
          },
          rB_LogCH_Mapping:
          {
            uLlogicalChannelIdentity: 1,
            dLlogicalChannelIdentity: 1,
            logicalChannelType: OMIT,
            cn_DomainIdentity: OMIT
          }
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 2
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          sS_rlc_Info:
          {
            sS_ul_RLC_Mode:
            [
              dl_AM_RLC_Mode:
              {
                inSequenceDelivery: GcTRUE,
                receivingWindowSize: rw32,
                dl_RLC_StatusInfo:
                {
                  timerStatusProhibit: tsp200,
                  timerEPC: OMIT,
                  missingPDU_Indicator: GcTRUE,
                  timerStatusPeriodic: OMIT
                }
              }
            ],
            sS_dl_RLC_Mode:
            {
              dl_PayloadSize: 128,
              dl_RLCModeInfo:
              [
                ul_AM_RLC_Mode:
                {
                  transmissionRLC_Discard:
                  [
                    noDiscard: dat15
                  ],
                  transmissionWindowSize: tw32,
                  timerRST: tr500,
                  max_RST: rst1,
                  pollingInfo:
                  {
                    timerPollProhibit: tpp200,
                    timerPoll: tp200,
                    poll_PDU: OMIT,
                    poll_SDU: sdu1,
                    lastTransmissionPDU_Poll: GcTRUE,
                    lastRetransmissionPDU_Poll: GcTRUE,
                    pollWindow: pw99,
                    timerPollPeriodic: OMIT
                  }
                }
              ]
            }
          },
          rB_LogCH_Mapping:
          {
            uLlogicalChannelIdentity: 2,
            dLlogicalChannelIdentity: 2,
            logicalChannelType: OMIT,
            cn_DomainIdentity: OMIT
          }
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 3
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          sS_rlc_Info:
          {
            sS_ul_RLC_Mode:
            [
              dl_AM_RLC_Mode:
              {
                inSequenceDelivery: GcTRUE,
                receivingWindowSize: rw32,
                dl_RLC_StatusInfo:
                {
                  timerStatusProhibit: tsp200,
                  timerEPC: OMIT,
                  missingPDU_Indicator: GcTRUE,
                  timerStatusPeriodic: OMIT
                }
              }
            ],
            sS_dl_RLC_Mode:
            {
              dl_PayloadSize: 128,
              dl_RLCModeInfo:
              [
                ul_AM_RLC_Mode:
                {
                  transmissionRLC_Discard:
                  [
                    noDiscard: dat15
                  ],
                  transmissionWindowSize: tw32,
                  timerRST: tr500,
                  max_RST: rst1,
                  pollingInfo:
                  {
                    timerPollProhibit: tpp200,
                    timerPoll: tp200,
                    poll_PDU: OMIT,
                    poll_SDU: sdu1,
                    lastTransmissionPDU_Poll: GcTRUE,
                    lastRetransmissionPDU_Poll: GcTRUE,
                    pollWindow: pw99,
                    timerPollPeriodic: OMIT
                  }
                }
              ]
            }
          },
          rB_LogCH_Mapping:
          {
            uLlogicalChannelIdentity: 3,
            dLlogicalChannelIdentity: 3,
            logicalChannelType: OMIT,
            cn_DomainIdentity: OMIT
          }
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 4
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          sS_rlc_Info:
          {
            sS_ul_RLC_Mode:
            [
              dl_AM_RLC_Mode:
              {
                inSequenceDelivery: GcTRUE,
                receivingWindowSize: rw32,
                dl_RLC_StatusInfo:
                {
                  timerStatusProhibit: tsp200,
                  timerEPC: OMIT,
                  missingPDU_Indicator: GcTRUE,
                  timerStatusPeriodic: OMIT
                }
              }
            ],
            sS_dl_RLC_Mode:
            {
              dl_PayloadSize: 128,
              dl_RLCModeInfo:
              [
                ul_AM_RLC_Mode:
                {
                  transmissionRLC_Discard:
                  [
                    noDiscard: dat15
                  ],
                  transmissionWindowSize: tw32,
                  timerRST: tr500,
                  max_RST: rst1,
                  pollingInfo:
                  {
                    timerPollProhibit: tpp200,
                    timerPoll: tp200,
                    poll_PDU: OMIT,
                    poll_SDU: sdu1,
                    lastTransmissionPDU_Poll: GcTRUE,
                    lastRetransmissionPDU_Poll: GcTRUE,
                    pollWindow: pw99,
                    timerPollPeriodic: OMIT
                  }
                }
              ]
            }
          },
          rB_LogCH_Mapping:
          {
            uLlogicalChannelIdentity: 4,
            dLlogicalChannelIdentity: 4,
            logicalChannelType: OMIT,
            cn_DomainIdentity: OMIT
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 27,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              noSegment: NULL
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 11,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              completeSIB_List:
              [
                {
                  sib_Type: systemInformationBlockType1,
                  sib_Data_variable: '1100010000000000000001011000100000101000000010100001000111100000000101000000000000000000000011000111010000'B
                },

                {
                  sib_Type: systemInformationBlockType2,
                  sib_Data_variable: '00000000000000000001'B
                }
              ]
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 11,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              completeSIB_List:
              [
                {
                  sib_Type: systemInformationBlockType1,
                  sib_Data_variable: '1100010000000000000001011000100000101000000010100001000111100000000101000000000000000000000011000111010000'B
                },

                {
                  sib_Type: systemInformationBlockType2,
                  sib_Data_variable: '00000000000000000001'B
                }
              ]
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 10,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              completeSIB_List:
              [
                {
                  sib_Type: systemInformationBlockType7,
                  sib_Data_variable: '100000101000000010000001'B
                },

                {
                  sib_Type: systemInformationBlockType3,
                  sib_Data_variable: '0100000000000000000000000000000010110111000110000000000000010000000000100100001000000100011111111111111111111111'B
                }
              ]
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 26,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              completeSIB_List:
              [
                {
                  sib_Type: systemInformationBlockType7,
                  sib_Data_variable: '100000101000000010000001'B
                },

                {
                  sib_Type: systemInformationBlockType4,
                  sib_Data_variable: '00000000000000000000000000000001011011100011000000000000001000000000010010000000000010001110111'B
                }
              ]
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 23,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              noSegment: NULL
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 19,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              firstSegment:
              {
                sib_Type: systemInformationBlockType5,
                seg_Count: 3,
                sib_Data_fixed: '000101010100010000111110000000001111111101000011111111111111110111010010000100001111000000101001000011000000101010100101010110000000000000001100110001011011010101111110001010111010000011111110100000111111101000001111111010'B
              }
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 21,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              subsequentSegment:
              {
                sib_Type: systemInformationBlockType5,
                segmentIndex: 1,
                sib_Data_fixed: '000011111111010000000000000000001101011000110100010000111111010011100101000001100001000011001010000000110000001110000001000000010110000010000000111000000000100010000110010000101001100100001010000000000011000000010001000101'B
              }
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 22,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              lastSegmentShort:
              {
                sib_Type: systemInformationBlockType5,
                segmentIndex: 2,
                sib_Data_variable: '1100101011010110100000000000011110001000011000000001011011011011011000100000000001000011000010001001010000001011011010000000010000'B
              }
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 3,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              completeSIB_List:
              [
                {
                  sib_Type: systemInformationBlockType6,
                  sib_Data_variable: '0000001010010001'B
                }
              ]
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 5,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              noSegment: NULL
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 6,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              noSegment: NULL
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 7,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              noSegment: NULL
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 2,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              completeSIB_List:
              [
                {
                  sib_Type: systemInformationBlockType7,
                  sib_Data_variable: '100000101000000010000001'B
                }
              ]
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 10,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              completeSIB_List:
              [
                {
                  sib_Type: systemInformationBlockType7,
                  sib_Data_variable: '100000101000000010000001'B
                },

                {
                  sib_Type: systemInformationBlockType3,
                  sib_Data_variable: '0100000000000000000000000000000010110111000110000000000000010000000000100100001000000100011111111111111111111111'B
                }
              ]
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 18,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              completeSIB_List:
              [
                {
                  sib_Type: systemInformationBlockType7,
                  sib_Data_variable: '100000101000000010000001'B
                },

                {
                  sib_Type: systemInformationBlockType18,
                  sib_Data_variable: '100010000001000000000010000000001'B
                }
              ]
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 26,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              completeSIB_List:
              [
                {
                  sib_Type: systemInformationBlockType7,
                  sib_Data_variable: '100000101000000010000001'B
                },

                {
                  sib_Type: systemInformationBlockType4,
                  sib_Data_variable: '00000000000000000000000000000001011011100011000000000000001000000000010010000000000010001110111'B
                }
              ]
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 31,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              noSegment: NULL
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 29,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              firstSegment:
              {
                sib_Type: systemInformationBlockType11,
                seg_Count: 2,
                sib_Data_fixed: '001000001101100100010010000000001000110010000100001000010010010110101000100000100110010001010011000001011001000010100111000010111000010100001000100010001100100101010100000001001010000101001010100001100001001010001000001010'B
              }
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 30,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              lastSegmentShort:
              {
                sib_Type: systemInformationBlockType11,
                segmentIndex: 1,
                sib_Data_variable: '000100001100001001010010011010101000011000010010101000101100011001010100101010100001001111101000100010000001010010110000100010100001010101111000'B
              }
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 13,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              completeSIB_List:
              [
                {
                  sib_Type: systemInformationBlockType12,
                  sib_Data_variable: '000000000'B
                }
              ]
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 14,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              noSegment: NULL
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 15,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              noSegment: NULL
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 18,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              completeSIB_List:
              [
                {
                  sib_Type: systemInformationBlockType7,
                  sib_Data_variable: '100000101000000010000001'B
                },

                {
                  sib_Type: systemInformationBlockType18,
                  sib_Data_variable: '100010000001000000000010000000001'B
                }
              ]
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 4,
        sg_POS: 1,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              completeSIB_List:
              [
                {
                  sib_Type: schedulingBlock1,
                  sib_Data_variable: '00010000101010001000001100110000010010010100111000101001110100000000010110100010001101110010100010010010'B
                }
              ]
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 3,
        sg_POS: 0,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              completeSIB_List:
              [
                {
                  sib_Type: masterInformationBlock,
                  sib_Data_variable: '0000000000000000010000000010010110101010000100010000000000001000100010110000101000100010110001001000100010100001101000100110100010001110010010010011000100010000'B
                }
              ]
            ]
          }
        }
      ]
    }

TTCN PDU: CPHY_Cell_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      tcell: 0,
      sfnOffset: 0,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      primaryScramblingCode_SS: 150,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      dLTxAttenuationLevel: 30
    }

TTCN PDU: CPHY_RL_Setup_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        physicalChannelIdentity: 0
      ],
      ratType: fdd,
      setupMessage:
      {
        physicalChannelInfo:
        [
          primaryCPICHInfo:
          {
            dl_TxPower_PCPICH: -60,
            txdiversityIndicator: GcFALSE
          }
        ]
      }
    }

TTCN PDU: CPHY_RL_Setup_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        physicalChannelIdentity: 1
      ],
      ratType: fdd,
      setupMessage:
      {
        physicalChannelInfo:
        [
          primarySCHInfo:
          {
            tstdIndicator: GcFALSE,
            dl_TxPower: -5
          }
        ]
      }
    }

TTCN PDU: CPHY_RL_Setup_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        physicalChannelIdentity: 2
      ],
      ratType: fdd,
      setupMessage:
      {
        physicalChannelInfo:
        [
          secondarySCHInfo:
          {
            tstdIndicator: GcFALSE,
            dl_TxPower: -5
          }
        ]
      }
    }

TTCN PDU: CPHY_RL_Setup_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        physicalChannelIdentity: 4
      ],
      ratType: fdd,
      setupMessage:
      {
        physicalChannelInfo:
        [
          primaryCCPCHInfo:
          {
            sttd_Indicator: GcFALSE,
            dl_TxPower: -2
          }
        ]
      }
    }

TTCN PDU: CPHY_TrCH_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        physicalChannelIdentity: 4
      ],
      ratType: fdd,
      trchConfigType:
      [
        nonDch: NULL
      ],
      configMessage:
      {
        activationTime:
        [
          activateNow: NULL
        ],
        ulconnectedTrCHList: OMIT,
        ulTFCS: OMIT,
        dlconnectedTrCHList:
        [
          {
            trchid: 11,
            dl_TransportChannelType: bch,
            transportChannelInfo:
            {
              tti:
              [
                tti20:
                [
                  {
                    tb_Size: 246,
                    numberOfTbSizeList:
                    [
                      [
                        one: NULL
                      ]
                    ],
                    logicalChannelList:
                    [
                      configured: NULL
                    ]
                  }
                ]
              ],
              semistaticTF_Information:
              {
                channelCodingType:
                [
                  convolutional: half
                ],
                rateMatchingAttribute# 1 # crc_Size# crc16
              }
            }
          }
        ]
        # dlTFCS#
        [
          normalTFCI_Signalling#
          [
            complete#
            {
              ctfcSize#
              [
                ctfc2Bit#
                [
                  {
                    ctfc2# 0 # powerOffsetInformation#
                    {
                      gainFactorInformation#
                      [
                        signalledGainFactors#
                        {
                          modeSpecificInfo#
                          [
                            fdd#
                            {
                              gainFactorBetaC# 11
                            }
                          ]
                          # gainFactorBetaD# 15 # referenceTFC_ID# 0
                        }
                      ]
                      # powerOffsetPp_m# OMIT
                    }
                  }
                ]
              ]
            }
          ]
        ]
      }
    }

TTCN PDU: CPHY_TrCH_Config_CNF

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        physicalChannelIdentity: 4
      ]
    }

TTCN PDU: CMAC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        physicalChannelIdentity: 4
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          activationTime:
          [
            activateNow: NULL
          ],
          uE_Info:
          {
            u_RNTI: OMIT,
            c_RNTI: OMIT
          },
          trCHInfo:
          {
            ulconnectedTrCHList: OMIT,
            ulTFCS: OMIT,
            dlconnectedTrCHList:
            [
              {
                trchid: 11,
                transportChannelInfo:
                {
                  tti:
                  [
                    tti20:
                    [
                      {
                        tb_Size: 246,
                        numberOfTbSizeList:
                        [
                          [
                            one: NULL
                          ]
                        ],
                        logicalChannelList:
                        [
                          configured: NULL
                        ]
                      }
                    ]
                  ],
                  semistaticTF_Information:
                  {
                    channelCodingType:
                    [
                      convolutional: half
                    ],
                    rateMatchingAttribute# 1 # crc_Size# crc16
                  }
                }
              }
            ]
            # dlTFCS#
            [
              normalTFCI_Signalling#
              [
                complete#
                {
                  ctfcSize#
                  [
                    ctfc2Bit#
                    [
                      {
                        ctfc2# 0 # powerOffsetInformation#
                        {
                          gainFactorInformation#
                          [
                            signalledGainFactors#
                            {
                              modeSpecificInfo#
                              [
                                fdd#
                                {
                                  gainFactorBetaC# 11
                                }
                              ]
                              # gainFactorBetaD# 15 # referenceTFC_ID# 0
                            }
                          ]
                          # powerOffsetPp_m# OMIT
                        }
                      }
                    ]
                  ]
                }
              ]
            ]
          }
          # trCH_LogCHMapping#
          {
            ulconnectedTrCHList# OMIT# dlconnectedTrCHList#
            [
              {
                trchid# 11 # trCH_LogCHMappingList#
                [
                  {
                    logicalChannel_Mapping#
                    [
                      dl_LogicalChannelMapping#
                      {
                        macHeaderManipulation# normalMacHeader# dl_TransportChannelType# bch# logicalChannelIdentity# 1 # logicalChannelType# bCCH# rlc_SizeList#
                        [
                          configured# NULL
                        ]
                        # mac_LogicalChannelPriority# 1
                      }
                    ]
                    # rB_Identity# #1 # cn_DomainIdentity# OMIT
                  }
                ]
              }
            ]
          }
        }
      ]
    }

TTCN PDU: CPHY_RL_Setup_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        physicalChannelIdentity: 5
      ],
      ratType: fdd,
      setupMessage:
      {
        physicalChannelInfo:
        [
          secondaryCCPCHInfo:
          {
            scramblingCode: 0,
            dl_ChannelizationCode:
            [
              sf64: 1
            ],
            sCCPCHSlotFormat: 8,
            timingOffset: 0,
            positionFixedOrFlexible: flexible,
            sttd_Indicator: GcFALSE,
            dl_TxPower: -2,
            powerOffsetOfTFCI_PO1: 6,
            powerOffsetOfPILOT_PO3: 6
          }
        ]
      }
    }

TTCN PDU: CPHY_TrCH_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        physicalChannelIdentity: 5
      ],
      ratType: fdd,
      trchConfigType:
      [
        nonDch: NULL
      ],
      configMessage:
      {
        activationTime:
        [
          activateNow: NULL
        ],
        ulconnectedTrCHList: OMIT,
        ulTFCS: OMIT,
        dlconnectedTrCHList:
        [
          {
            trchid: 12,
            dl_TransportChannelType: pch,
            transportChannelInfo:
            {
              tti:
              [
                tti10:
                [
                  {
                    tb_Size: 240,
                    numberOfTbSizeList:
                    [
                      [
                        zero: NULL
                      ],

                      [
                        one: NULL
                      ]
                    ],
                    logicalChannelList:
                    [
                      allSizes: NULL
                    ]
                  }
                ]
              ],
              semistaticTF_Information:
              {
                channelCodingType:
                [
                  convolutional: half
                ],
                rateMatchingAttribute# 230 # crc_Size# crc16
              }
            }
          }
          #
          {
            trchid# 13 # dl_TransportChannelType# fach# transportChannelInfo#
            {
              tti#
              [
                tti10#
                [
                  {
                    tb_Size# 168 # numberOfTbSizeList#
                    [
                      [
                        zero# NULL
                      ]
                      #
                      [
                        one# NULL
                      ]
                      #
                      [
                        small# 2
                      ]
                    ]
                    # logicalChannelList#
                    [
                      allSizes# NULL
                    ]
                  }
                ]
              ]
              # semistaticTF_Information#
              {
                channelCodingType#
                [
                  convolutional# half
                ]
                # rateMatchingAttribute# 220 # crc_Size# crc16
              }
            }
          }
          #
          {
            trchid# 14 # dl_TransportChannelType# fach# transportChannelInfo#
            {
              tti#
              [
                tti10#
                [
                  {
                    tb_Size# 360 # numberOfTbSizeList#
                    [
                      [
                        zero# NULL
                      ]
                      #
                      [
                        one# NULL
                      ]
                    ]
                    # logicalChannelList#
                    [
                      allSizes# NULL
                    ]
                  }
                ]
              ]
              # semistaticTF_Information#
              {
                channelCodingType#
                [
                  turbo# NULL
                ]
                # rateMatchingAttribute# 130 # crc_Size# crc16
              }
            }
          }
        ]
        # dlTFCS#
        [
          normalTFCI_Signalling#
          [
            complete#
            {
              ctfcSize#
              [
                ctfc4Bit#
                [
                  {
                    ctfc4# 0 # powerOffsetInformation#
                    {
                      gainFactorInformation#
                      [
                        computedGainFactors# 0
                      ]
                      # powerOffsetPp_m# OMIT
                    }
                  }
                  #
                  {
                    ctfc4# 1 # powerOffsetInformation#
                    {
                      gainFactorInformation#
                      [
                        computedGainFactors# 0
                      ]
                      # powerOffsetPp_m# OMIT
                    }
                  }
                  #
                  {
                    ctfc4# 2 # powerOffsetInformation#
                    {
                      gainFactorInformation#
                      [
                        computedGainFactors# 0
                      ]
                      # powerOffsetPp_m# OMIT
                    }
                  }
                  #
                  {
                    ctfc4# 3 # powerOffsetInformation#
                    {
                      gainFactorInformation#
                      [
                        computedGainFactors# 0
                      ]
                      # powerOffsetPp_m# OMIT
                    }
                  }
                  #
                  {
                    ctfc4# 4 # powerOffsetInformation#
                    {
                      gainFactorInformation#
                      [
                        computedGainFactors# 0
                      ]
                      # powerOffsetPp_m# OMIT
                    }
                  }
                  #
                  {
                    ctfc4# 5 # powerOffsetInformation#
                    {
                      gainFactorInformation#
                      [
                        computedGainFactors# 0
                      ]
                      # powerOffsetPp_m# OMIT
                    }
                  }
                  #
                  {
                    ctfc4# 6 # powerOffsetInformation#
                    {
                      gainFactorInformation#
                      [
                        computedGainFactors# 0
                      ]
                      # powerOffsetPp_m# OMIT
                    }
                  }
                  #
                  {
                    ctfc4# 8 # powerOffsetInformation#
                    {
                      gainFactorInformation#
                      [
                        signalledGainFactors#
                        {
                          modeSpecificInfo#
                          [
                            fdd#
                            {
                              gainFactorBetaC# 11
                            }
                          ]
                          # gainFactorBetaD# 15 # referenceTFC_ID# 0
                        }
                      ]
                      # powerOffsetPp_m# OMIT
                    }
                  }
                ]
              ]
            }
          ]
        ]
      }
    }

TTCN PDU: CMAC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        physicalChannelIdentity: 5
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          activationTime:
          [
            activateNow: NULL
          ],
          uE_Info:
          {
            u_RNTI: OMIT,
            c_RNTI: OMIT
          },
          trCHInfo:
          {
            ulconnectedTrCHList: OMIT,
            ulTFCS: OMIT,
            dlconnectedTrCHList:
            [
              {
                trchid: 12,
                transportChannelInfo:
                {
                  tti:
                  [
                    tti10:
                    [
                      {
                        tb_Size: 240,
                        numberOfTbSizeList:
                        [
                          [
                            zero: NULL
                          ],

                          [
                            one: NULL
                          ]
                        ],
                        logicalChannelList:
                        [
                          allSizes: NULL
                        ]
                      }
                    ]
                  ],
                  semistaticTF_Information:
                  {
                    channelCodingType:
                    [
                      convolutional: half
                    ],
                    rateMatchingAttribute# 230 # crc_Size# crc16
                  }
                }
              }
              #
              {
                trchid# 13 # transportChannelInfo#
                {
                  tti#
                  [
                    tti10#
                    [
                      {
                        tb_Size# 168 # numberOfTbSizeList#
                        [
                          [
                            zero# NULL
                          ]
                          #
                          [
                            one# NULL
                          ]
                          #
                          [
                            small# 2
                          ]
                        ]
                        # logicalChannelList#
                        [
                          allSizes# NULL
                        ]
                      }
                    ]
                  ]
                  # semistaticTF_Information#
                  {
                    channelCodingType#
                    [
                      convolutional# half
                    ]
                    # rateMatchingAttribute# 220 # crc_Size# crc16
                  }
                }
              }
              #
              {
                trchid# 14 # transportChannelInfo#
                {
                  tti#
                  [
                    tti10#
                    [
                      {
                        tb_Size# 360 # numberOfTbSizeList#
                        [
                          [
                            zero# NULL
                          ]
                          #
                          [
                            one# NULL
                          ]
                        ]
                        # logicalChannelList#
                        [
                          allSizes# NULL
                        ]
                      }
                    ]
                  ]
                  # semistaticTF_Information#
                  {
                    channelCodingType#
                    [
                      turbo# NULL
                    ]
                    # rateMatchingAttribute# 130 # crc_Size# crc16
                  }
                }
              }
            ]
            # dlTFCS#
            [
              normalTFCI_Signalling#
              [
                complete#
                {
                  ctfcSize#
                  [
                    ctfc4Bit#
                    [
                      {
                        ctfc4# 0 # powerOffsetInformation#
                        {
                          gainFactorInformation#
                          [
                            computedGainFactors# 0
                          ]
                          # powerOffsetPp_m# OMIT
                        }
                      }
                      #
                      {
                        ctfc4# 1 # powerOffsetInformation#
                        {
                          gainFactorInformation#
                          [
                            computedGainFactors# 0
                          ]
                          # powerOffsetPp_m# OMIT
                        }
                      }
                      #
                      {
                        ctfc4# 2 # powerOffsetInformation#
                        {
                          gainFactorInformation#
                          [
                            computedGainFactors# 0
                          ]
                          # powerOffsetPp_m# OMIT
                        }
                      }
                      #
                      {
                        ctfc4# 3 # powerOffsetInformation#
                        {
                          gainFactorInformation#
                          [
                            computedGainFactors# 0
                          ]
                          # powerOffsetPp_m# OMIT
                        }
                      }
                      #
                      {
                        ctfc4# 4 # powerOffsetInformation#
                        {
                          gainFactorInformation#
                          [
                            computedGainFactors# 0
                          ]
                          # powerOffsetPp_m# OMIT
                        }
                      }
                      #
                      {
                        ctfc4# 5 # powerOffsetInformation#
                        {
                          gainFactorInformation#
                          [
                            computedGainFactors# 0
                          ]
                          # powerOffsetPp_m# OMIT
                        }
                      }
                      #
                      {
                        ctfc4# 6 # powerOffsetInformation#
                        {
                          gainFactorInformation#
                          [
                            computedGainFactors# 0
                          ]
                          # powerOffsetPp_m# OMIT
                        }
                      }
                      #
                      {
                        ctfc4# 8 # powerOffsetInformation#
                        {
                          gainFactorInformation#
                          [
                            signalledGainFactors#
                            {
                              modeSpecificInfo#
                              [
                                fdd#
                                {
                                  gainFactorBetaC# 11
                                }
                              ]
                              # gainFactorBetaD# 15 # referenceTFC_ID# 0
                            }
                          ]
                          # powerOffsetPp_m# OMIT
                        }
                      }
                    ]
                  ]
                }
              ]
            ]
          }
          # trCH_LogCHMapping#
          {
            ulconnectedTrCHList# OMIT# dlconnectedTrCHList#
            [
              {
                trchid# 12 # trCH_LogCHMappingList#
                [
                  {
                    logicalChannel_Mapping#
                    [
                      dl_LogicalChannelMapping#
                      {
                        macHeaderManipulation# normalMacHeader# dl_TransportChannelType# pch# logicalChannelIdentity# 1 # logicalChannelType# pCCH# rlc_SizeList#
                        [
                          configured# NULL
                        ]
                        # mac_LogicalChannelPriority# 1
                      }
                    ]
                    # rB_Identity# #2 # cn_DomainIdentity# OMIT
                  }
                ]
              }
              #
              {
                trchid# 13 # trCH_LogCHMappingList#
                [
                  {
                    logicalChannel_Mapping#
                    [
                      dl_LogicalChannelMapping#
                      {
                        macHeaderManipulation# normalMacHeader# dl_TransportChannelType# fach# logicalChannelIdentity# 5 # logicalChannelType# cCCH# rlc_SizeList#
                        [
                          configured# NULL
                        ]
                        # mac_LogicalChannelPriority# 1
                      }
                    ]
                    # rB_Identity# 0 # cn_DomainIdentity# OMIT
                  }
                ]
              }
            ]
          }
        }
      ]
    }

TTCN PDU: CPHY_RL_Setup_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        physicalChannelIdentity: 6
      ],
      ratType: fdd,
      setupMessage:
      {
        physicalChannelInfo:
        [
          pICHInfo:
          {
            pichinfo:
            [
              fdd:
              {
                channelisationCode256: 2,
                pi_CountPerFrame: e18,
                sttd_Indicator: GcFALSE
              }
            ],
            dl_TxPower: -5,
            sccpchId_associated: 5
          }
        ]
      }
    }

TTCN PDU: CPHY_RL_Setup_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        physicalChannelIdentity: 7
      ],
      ratType: fdd,
      setupMessage:
      {
        physicalChannelInfo:
        [
          aICHInfo:
          {
            aichinfo:
            {
              channelisationCode256: 3,
              sttd_Indicator: GcFALSE,
              aich_TransmissionTiming: e0
            },
            dl_TxPower: -5
          }
        ]
      }
    }

TTCN PDU: CPHY_RL_Setup_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        physicalChannelIdentity: 8
      ],
      ratType: fdd,
      setupMessage:
      {
        physicalChannelInfo:
        [
          pRACHInfo:
          {
            fdd_tdd:
            [
              fdd:
              {
                preambleSignature: '0000000011111111'B,
                spreadingFactorForDataPart: sfpr64,
                preambleScramblingCode: 0,
                puncturingLimit: pl1,
                accessSlot: '111111111111'B
              }
            ]
          }
        ]
      }
    }

TTCN PDU: CPHY_TrCH_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        physicalChannelIdentity: 8
      ],
      ratType: fdd,
      trchConfigType:
      [
        nonDch: NULL
      ],
      configMessage:
      {
        activationTime:
        [
          activateNow: NULL
        ],
        ulconnectedTrCHList:
        [
          {
            trchid: 15,
            ul_TransportChannelType: rach,
            transportChannelInfo:
            {
              tti:
              [
                tti20:
                [
                  {
                    tb_Size: 168,
                    numberOfTbSizeList:
                    [
                      [
                        one: NULL
                      ]
                    ],
                    logicalChannelList:
                    [
                      configured: NULL
                    ]
                  },

                  {
                    tb_Size: 360,
                    numberOfTbSizeList:
                    [
                      [
                        one: NULL
                      ]
                    ],
                    logicalChannelList:
                    [
                      configured: NULL
                    ]
                  }
                ]
              ],
              semistaticTF_Information:
              {
                channelCodingType:
                [
                  convolutional: half
                ],
                rateMatchingAttribute# 150 # crc_Size# crc16
              }
            }
          }
        ]
        # ulTFCS#
        [
          normalTFCI_Signalling#
          [
            complete#
            {
              ctfcSize#
              [
                ctfc2Bit#
                [
                  {
                    ctfc2# 0 # powerOffsetInformation# OMIT
                  }
                  #
                  {
                    ctfc2# 1 # powerOffsetInformation# OMIT
                  }
                ]
              ]
            }
          ]
        ]
        # dlconnectedTrCHList# OMIT# dlTFCS# OMIT
      }
    }

TTCN PDU: CMAC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        physicalChannelIdentity: 8
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          activationTime:
          [
            activateNow: NULL
          ],
          uE_Info:
          {
            u_RNTI: OMIT,
            c_RNTI: OMIT
          },
          trCHInfo:
          {
            ulconnectedTrCHList:
            [
              {
                trchid: 15,
                transportChannelInfo:
                {
                  tti:
                  [
                    tti20:
                    [
                      {
                        tb_Size: 168,
                        numberOfTbSizeList:
                        [
                          [
                            one: NULL
                          ]
                        ],
                        logicalChannelList:
                        [
                          configured: NULL
                        ]
                      },

                      {
                        tb_Size: 360,
                        numberOfTbSizeList:
                        [
                          [
                            one: NULL
                          ]
                        ],
                        logicalChannelList:
                        [
                          configured: NULL
                        ]
                      }
                    ]
                  ],
                  semistaticTF_Information:
                  {
                    channelCodingType:
                    [
                      convolutional: half
                    ],
                    rateMatchingAttribute# 150 # crc_Size# crc16
                  }
                }
              }
            ]
            # ulTFCS#
            [
              normalTFCI_Signalling#
              [
                complete#
                {
                  ctfcSize#
                  [
                    ctfc2Bit#
                    [
                      {
                        ctfc2# 0 # powerOffsetInformation# OMIT
                      }
                      #
                      {
                        ctfc2# 1 # powerOffsetInformation# OMIT
                      }
                    ]
                  ]
                }
              ]
            ]
            # dlconnectedTrCHList# OMIT# dlTFCS# OMIT
          }
          # trCH_LogCHMapping#
          {
            ulconnectedTrCHList#
            [
              {
                trchid# 15 # trCH_LogCHMappingList#
                [
                  {
                    logicalChannel_Mapping#
                    [
                      ul_LogicalChannelMapping#
                      {
                        macHeaderManipulation# normalMacHeader# ul_TransportChannelType# rach# logicalChannelIdentity# 5 # logicalChannelType# cCCH
                      }
                    ]
                    # rB_Identity# 0 # cn_DomainIdentity# OMIT
                  }
                ]
              }
            ]
            # dlconnectedTrCHList# OMIT
          }
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          sS_rlc_Info:
          {
            sS_ul_RLC_Mode: OMIT,
            sS_dl_RLC_Mode:
            {
              dl_PayloadSize: 246,
              dl_RLCModeInfo:
              [
                ul_TM_RLC_Mode:
                {
                  transmissionRLC_Discard: OMIT,
                  segmentationIndication: GcFALSE
                }
              ]
            }
          },
          rB_LogCH_Mapping:
          {
            uLlogicalChannelIdentity: OMIT,
            dLlogicalChannelIdentity: 1,
            logicalChannelType: OMIT,
            cn_DomainIdentity: OMIT
          }
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        rB_Identity: -2
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          sS_rlc_Info:
          {
            sS_ul_RLC_Mode: OMIT,
            sS_dl_RLC_Mode:
            {
              dl_PayloadSize: 240,
              dl_RLCModeInfo:
              [
                ul_TM_RLC_Mode:
                {
                  transmissionRLC_Discard: OMIT,
                  segmentationIndication: GcFALSE
                }
              ]
            }
          },
          rB_LogCH_Mapping:
          {
            uLlogicalChannelIdentity: OMIT,
            dLlogicalChannelIdentity: 1,
            logicalChannelType: OMIT,
            cn_DomainIdentity: OMIT
          }
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        rB_Identity: 0
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          sS_rlc_Info:
          {
            sS_ul_RLC_Mode: OMIT,
            sS_dl_RLC_Mode:
            {
              dl_PayloadSize: 152,
              dl_RLCModeInfo:
              [
                ul_UM_RLC_Mode:
                {
                  transmissionRLC_Discard:
                  [
                    timerBasedNoExplicit: dt100
                  ]
                }
              ]
            }
          },
          rB_LogCH_Mapping:
          {
            uLlogicalChannelIdentity: OMIT,
            dLlogicalChannelIdentity: 5,
            logicalChannelType: OMIT,
            cn_DomainIdentity: OMIT
          }
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        rB_Identity: 0
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          sS_rlc_Info:
          {
            sS_ul_RLC_Mode:
            [
              dl_TM_RLC_Mode:
              {
                segmentationIndication: GcFALSE
              }
            ],
            sS_dl_RLC_Mode:
            {
              dl_PayloadSize: 166,
              dl_RLCModeInfo:
              [
                ul_TM_RLC_Mode:
                {
                  transmissionRLC_Discard: OMIT,
                  segmentationIndication: GcFALSE
                }
              ]
            }
          },
          rB_LogCH_Mapping:
          {
            uLlogicalChannelIdentity: 5,
            dLlogicalChannelIdentity: OMIT,
            logicalChannelType: OMIT,
            cn_DomainIdentity: OMIT
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 27,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              noSegment: NULL
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 11,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              completeSIB_List:
              [
                {
                  sib_Type: systemInformationBlockType1,
                  sib_Data_variable: '1100010000000000000001011000100000010000000010100001000000000000000001000000000000000000000011000111010000'B
                },

                {
                  sib_Type: systemInformationBlockType2,
                  sib_Data_variable: '00000000000000000001'B
                }
              ]
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 11,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              completeSIB_List:
              [
                {
                  sib_Type: systemInformationBlockType1,
                  sib_Data_variable: '1100010000000000000001011000100000010000000010100001000000000000000001000000000000000000000011000111010000'B
                },

                {
                  sib_Type: systemInformationBlockType2,
                  sib_Data_variable: '00000000000000000001'B
                }
              ]
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 10,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              completeSIB_List:
              [
                {
                  sib_Type: systemInformationBlockType7,
                  sib_Data_variable: '100000101000000010000001'B
                },

                {
                  sib_Type: systemInformationBlockType3,
                  sib_Data_variable: '0100000000000000000000000000010010110111000110000000000000010000000000100100001000000100011111111111111111111111'B
                }
              ]
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 26,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              completeSIB_List:
              [
                {
                  sib_Type: systemInformationBlockType7,
                  sib_Data_variable: '100000101000000010000001'B
                },

                {
                  sib_Type: systemInformationBlockType4,
                  sib_Data_variable: '00000000000000000000000000001001011011100011000000000000001000000000010010000000000010001110111'B
                }
              ]
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 23,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              noSegment: NULL
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 19,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              firstSegment:
              {
                sib_Type: systemInformationBlockType5,
                seg_Count: 3,
                sib_Data_fixed: '000101010100010000111110000000001111111101000011111111111111110111010010000100001111000000101001000011000000101010100101010110000000000000001100110001011011010101111110001010111010000011111110100000111111101000001111111010'B
              }
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 21,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              subsequentSegment:
              {
                sib_Type: systemInformationBlockType5,
                segmentIndex: 1,
                sib_Data_fixed: '000011111111010000000000000000001101011000110100010000111111010011100101000001100001000011001010000000110000001110000001000000010110000010000000111000000000100010000110010000101001100100001010000000000011000000010001000101'B
              }
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 22,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              lastSegmentShort:
              {
                sib_Type: systemInformationBlockType5,
                segmentIndex: 2,
                sib_Data_variable: '1100101011010110100000000000011110001000011000000001011011011011011000100000000001000011000010001001010000001011011010000000010000'B
              }
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 3,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              completeSIB_List:
              [
                {
                  sib_Type: systemInformationBlockType6,
                  sib_Data_variable: '0000001010010001'B
                }
              ]
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 5,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              noSegment: NULL
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 6,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              noSegment: NULL
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 7,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              noSegment: NULL
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 2,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              completeSIB_List:
              [
                {
                  sib_Type: systemInformationBlockType7,
                  sib_Data_variable: '100000101000000010000001'B
                }
              ]
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 10,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              completeSIB_List:
              [
                {
                  sib_Type: systemInformationBlockType7,
                  sib_Data_variable: '100000101000000010000001'B
                },

                {
                  sib_Type: systemInformationBlockType3,
                  sib_Data_variable: '0100000000000000000000000000010010110111000110000000000000010000000000100100001000000100011111111111111111111111'B
                }
              ]
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 18,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              completeSIB_List:
              [
                {
                  sib_Type: systemInformationBlockType7,
                  sib_Data_variable: '100000101000000010000001'B
                },

                {
                  sib_Type: systemInformationBlockType18,
                  sib_Data_variable: '100010000001000000000010000000001'B
                }
              ]
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 26,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              completeSIB_List:
              [
                {
                  sib_Type: systemInformationBlockType7,
                  sib_Data_variable: '100000101000000010000001'B
                },

                {
                  sib_Type: systemInformationBlockType4,
                  sib_Data_variable: '00000000000000000000000000001001011011100011000000000000001000000000010010000000000010001110111'B
                }
              ]
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 31,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              noSegment: NULL
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 29,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              firstSegment:
              {
                sib_Type: systemInformationBlockType11,
                seg_Count: 2,
                sib_Data_fixed: '001000001101100100010010000100001001001011000100000000010001100100101000100000100110010001010011000001011001000010100111000010111000010100001000100010001100100101010100000001001010000101001010100001100001001010001000001010'B
              }
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 30,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              lastSegmentShort:
              {
                sib_Type: systemInformationBlockType11,
                segmentIndex: 1,
                sib_Data_variable: '000100001100001001010010011010101000011000010010101000101100011001010100101010100001001111101000100010000001010010110000100010100001010101111000'B
              }
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 13,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              completeSIB_List:
              [
                {
                  sib_Type: systemInformationBlockType12,
                  sib_Data_variable: '000000000'B
                }
              ]
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 14,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              noSegment: NULL
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 15,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              noSegment: NULL
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 18,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              completeSIB_List:
              [
                {
                  sib_Type: systemInformationBlockType7,
                  sib_Data_variable: '100000101000000010000001'B
                },

                {
                  sib_Type: systemInformationBlockType18,
                  sib_Data_variable: '100010000001000000000010000000001'B
                }
              ]
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 4,
        sg_POS: 1,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              completeSIB_List:
              [
                {
                  sib_Type: schedulingBlock1,
                  sib_Data_variable: '00010000101100001000001100110000010010010101011000101001110100000000010111000010001101110011000010010010'B
                }
              ]
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 3,
        sg_POS: 0,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              completeSIB_List:
              [
                {
                  sib_Type: masterInformationBlock,
                  sib_Data_variable: '0001000000000000010000000010010110101100000100010000000000010000100010110000110000100010110001010000100010100001110000100110100010010110010010010011000100010000'B
                }
              ]
            ]
          }
        }
      ]
    }

TTCN PDU: RLC_TR_DATA_IND

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: 0
      ],
      tM_message:
      [
        uL_CCCH_Message: PDU:
        {
          integrityCheckInfo: OMIT,
          message:
          [
            rrcConnectionRequest:
            {
              initialUE_Identity:
              [
                p_TMSI_and_RAI:
                {
                  p_TMSI: '00010010001101000101011001111000'B,
                  rai:
                  {
                    lai:
                    {
                      plmn_Identity:
                      {
                        mcc:
                        [
                          0,
                          0,
                          1
                        ],
                        mnc:
                        [
                          0,
                          1
                        ]
                      },
                      lac: '0000000000000010'B
                    },
                    rac: '00000101'B
                  }
                }
              ],
              establishmentCause: registration,
              protocolErrorIndicator: noError,
              measuredResultsOnRACH: OMIT,
              v3d0NonCriticalExtensions: OMIT
            }
          ]
        }
      ]
    }

TTCN PDU: RLC_UM_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: 0
      ],
      uM_message:
      [
        dL_CCCH_Message: PDU:
        {
          integrityCheckInfo: OMIT,
          message:
          [
            rrcConnectionSetup:
            [
              r3:
              {
                rrcConnectionSetup_r3:
                {
                  initialUE_Identity:
                  [
                    p_TMSI_and_RAI:
                    {
                      p_TMSI: '00010010001101000101011001111000'B,
                      rai:
                      {
                        lai:
                        {
                          plmn_Identity:
                          {
                            mcc:
                            [
                              0,
                              0,
                              1
                            ],
                            mnc:
                            [
                              0,
                              1
                            ]
                          },
                          lac: '0000000000000010'B
                        },
                        rac: '00000101'B
                      }
                    }
                  ],
                  rrc_TransactionIdentifier: 0,
                  activationTime: OMIT,
                  new_U_RNTI:
                  {
                    srnc_Identity: '000000000001'B,
                    s_RNTI: '00000000000000000001'B
                  },
                  new_c_RNTI: OMIT,
                  rrc_StateIndicator: cell_DCH,
                  utran_DRX_CycleLengthCoeff: 9,
                  capabilityUpdateRequirement:
                  {
                    ue_RadioCapabilityFDDUpdateRequirement: GcTRUE,
                    ue_RadioCapabilityTDDUpdateRequirement: GcFALSE,
                    systemSpecificCapUpdateReqList:
                    [
                      gsm
                    ]
                  },
                  srb_InformationSetupList:
                  [
                    {
                      rb_Identity: OMIT,
                      rlc_InfoChoice:
                      [
                        rlc_Info:
                        {
                          ul_RLC_Mode:
                          [
                            ul_UM_RLC_Mode:
                            {
                              transmissionRLC_Discard: OMIT
                            }
                          ],
                          dl_RLC_Mode:
                          [
                            dl_UM_RLC_Mode: NULL
                          ]
                        }
                      ],
                      rb_MappingInfo:
                      [
                        {
                          ul_LogicalChannelMappings:
                          [
                            oneLogicalChannel:
                            {
                              ul_TransportChannelType:
                              [
                                dch: 5
                              ],
                              logicalChannelIdentity: 1,
                              rlc_SizeList:
                              [
                                configured: NULL
                              ],
                              mac_LogicalChannelPriority: 1
                            }
                          ],
                          dl_LogicalChannelMappingList:
                          [
                            {
                              dl_TransportChannelType:
                              [
                                dch: 10
                              ],
                              logicalChannelIdentity: 1
                            }
                          ]
                        },

                        {
                          ul_LogicalChannelMappings:
                          [
                            oneLogicalChannel:
                            {
                              ul_TransportChannelType:
                              [
                                rach: NULL
                              ],
                              logicalChannelIdentity: 1,
                              rlc_SizeList:
                              [
                                explicitList:
                                [
                                  {
                                    rlc_SizeIndex: 1
                                  }
                                ]
                              ],
                              mac_LogicalChannelPriority: 1
                            }
                          ],
                          dl_LogicalChannelMappingList:
                          [
                            {
                              dl_TransportChannelType:
                              [
                                fach: NULL
                              ],
                              logicalChannelIdentity: 1
                            }
                          ]
                        }
                      ]
                    },

                    {
                      rb_Identity: OMIT,
                      rlc_InfoChoice:
                      [
                        rlc_Info:
                        {
                          ul_RLC_Mode:
                          [
                            ul_AM_RLC_Mode:
                            {
                              transmissionRLC_Discard:
                              [
                                noDiscard: dat15
                              ],
                              transmissionWindowSize: tw32,
                              timerRST: tr500,
                              max_RST: rst1,
                              pollingInfo:
                              {
                                timerPollProhibit: tpp200,
                                timerPoll: tp200,
                                poll_PDU: OMIT,
                                poll_SDU: sdu1,
                                lastTransmissionPDU_Poll: GcTRUE,
                                lastRetransmissionPDU_Poll: GcTRUE,
                                pollWindow: pw99,
                                timerPollPeriodic: OMIT
                              }
                            }
                          ],
                          dl_RLC_Mode:
                          [
                            dl_AM_RLC_Mode:
                            {
                              inSequenceDelivery: GcTRUE,
                              receivingWindowSize: rw32,
                              dl_RLC_StatusInfo:
                              {
                                timerStatusProhibit: tsp200,
                                timerEPC: OMIT,
                                missingPDU_Indicator: GcTRUE,
                                timerStatusPeriodic: OMIT
                              }
                            }
                          ]
                        }
                      ],
                      rb_MappingInfo:
                      [
                        {
                          ul_LogicalChannelMappings:
                          [
                            oneLogicalChannel:
                            {
                              ul_TransportChannelType:
                              [
                                dch: 5
                              ],
                              logicalChannelIdentity: 2,
                              rlc_SizeList:
                              [
                                configured: NULL
                              ],
                              mac_LogicalChannelPriority: 2
                            }
                          ],
                          dl_LogicalChannelMappingList:
                          [
                            {
                              dl_TransportChannelType:
                              [
                                dch: 10
                              ],
                              logicalChannelIdentity: 2
                            }
                          ]
                        },

                        {
                          ul_LogicalChannelMappings:
                          [
                            oneLogicalChannel:
                            {
                              ul_TransportChannelType:
                              [
                                rach: NULL
                              ],
                              logicalChannelIdentity: 2,
                              rlc_SizeList:
                              [
                                explicitList:
                                [
                                  {
                                    rlc_SizeIndex: 1
                                  }
                                ]
                              ],
                              mac_LogicalChannelPriority: 2
                            }
                          ],
                          dl_LogicalChannelMappingList:
                          [
                            {
                              dl_TransportChannelType:
                              [
                                fach: NULL
                              ],
                              logicalChannelIdentity: 2
                            }
                          ]
                        }
                      ]
                    },

                    {
                      rb_Identity: OMIT,
                      rlc_InfoChoice:
                      [
                        rlc_Info:
                        {
                          ul_RLC_Mode:
                          [
                            ul_AM_RLC_Mode:
                            {
                              transmissionRLC_Discard:
                              [
                                noDiscard: dat15
                              ],
                              transmissionWindowSize: tw32,
                              timerRST: tr500,
                              max_RST: rst1,
                              pollingInfo:
                              {
                                timerPollProhibit: tpp200,
                                timerPoll: tp200,
                                poll_PDU: OMIT,
                                poll_SDU: sdu1,
                                lastTransmissionPDU_Poll: GcTRUE,
                                lastRetransmissionPDU_Poll: GcTRUE,
                                pollWindow: pw99,
                                timerPollPeriodic: OMIT
                              }
                            }
                          ],
                          dl_RLC_Mode:
                          [
                            dl_AM_RLC_Mode:
                            {
                              inSequenceDelivery: GcTRUE,
                              receivingWindowSize: rw32,
                              dl_RLC_StatusInfo:
                              {
                                timerStatusProhibit: tsp200,
                                timerEPC: OMIT,
                                missingPDU_Indicator: GcTRUE,
                                timerStatusPeriodic: OMIT
                              }
                            }
                          ]
                        }
                      ],
                      rb_MappingInfo:
                      [
                        {
                          ul_LogicalChannelMappings:
                          [
                            oneLogicalChannel:
                            {
                              ul_TransportChannelType:
                              [
                                dch: 5
                              ],
                              logicalChannelIdentity: 3,
                              rlc_SizeList:
                              [
                                configured: NULL
                              ],
                              mac_LogicalChannelPriority: 3
                            }
                          ],
                          dl_LogicalChannelMappingList:
                          [
                            {
                              dl_TransportChannelType:
                              [
                                dch: 10
                              ],
                              logicalChannelIdentity: 3
                            }
                          ]
                        },

                        {
                          ul_LogicalChannelMappings:
                          [
                            oneLogicalChannel:
                            {
                              ul_TransportChannelType:
                              [
                                rach: NULL
                              ],
                              logicalChannelIdentity: 3,
                              rlc_SizeList:
                              [
                                explicitList:
                                [
                                  {
                                    rlc_SizeIndex: 1
                                  }
                                ]
                              ],
                              mac_LogicalChannelPriority: 3
                            }
                          ],
                          dl_LogicalChannelMappingList:
                          [
                            {
                              dl_TransportChannelType:
                              [
                                fach: NULL
                              ],
                              logicalChannelIdentity: 3
                            }
                          ]
                        }
                      ]
                    },

                    {
                      rb_Identity: OMIT,
                      rlc_InfoChoice:
                      [
                        rlc_Info:
                        {
                          ul_RLC_Mode:
                          [
                            ul_AM_RLC_Mode:
                            {
                              transmissionRLC_Discard:
                              [
                                noDiscard: dat15
                              ],
                              transmissionWindowSize: tw32,
                              timerRST: tr500,
                              max_RST: rst1,
                              pollingInfo:
                              {
                                timerPollProhibit: tpp200,
                                timerPoll: tp200,
                                poll_PDU: OMIT,
                                poll_SDU: sdu1,
                                lastTransmissionPDU_Poll: GcTRUE,
                                lastRetransmissionPDU_Poll: GcTRUE,
                                pollWindow: pw99,
                                timerPollPeriodic: OMIT
                              }
                            }
                          ],
                          dl_RLC_Mode:
                          [
                            dl_AM_RLC_Mode:
                            {
                              inSequenceDelivery: GcTRUE,
                              receivingWindowSize: rw32,
                              dl_RLC_StatusInfo:
                              {
                                timerStatusProhibit: tsp200,
                                timerEPC: OMIT,
                                missingPDU_Indicator: GcTRUE,
                                timerStatusPeriodic: OMIT
                              }
                            }
                          ]
                        }
                      ],
                      rb_MappingInfo:
                      [
                        {
                          ul_LogicalChannelMappings:
                          [
                            oneLogicalChannel:
                            {
                              ul_TransportChannelType:
                              [
                                dch: 5
                              ],
                              logicalChannelIdentity: 4,
                              rlc_SizeList:
                              [
                                configured: NULL
                              ],
                              mac_LogicalChannelPriority: 4
                            }
                          ],
                          dl_LogicalChannelMappingList:
                          [
                            {
                              dl_TransportChannelType:
                              [
                                dch: 10
                              ],
                              logicalChannelIdentity: 4
                            }
                          ]
                        },

                        {
                          ul_LogicalChannelMappings:
                          [
                            oneLogicalChannel:
                            {
                              ul_TransportChannelType:
                              [
                                rach: NULL
                              ],
                              logicalChannelIdentity: 4,
                              rlc_SizeList:
                              [
                                explicitList:
                                [
                                  {
                                    rlc_SizeIndex: 1
                                  }
                                ]
                              ],
                              mac_LogicalChannelPriority: 4
                            }
                          ],
                          dl_LogicalChannelMappingList:
                          [
                            {
                              dl_TransportChannelType:
                              [
                                fach: NULL
                              ],
                              logicalChannelIdentity: 4
                            }
                          ]
                        }
                      ]
                    }
                  ],
                  ul_CommonTransChInfo:
                  {
                    tfc_Subset: OMIT,
                    prach_TFCS: OMIT,
                    modeSpecificInfo:
                    [
                      fdd:
                      {
                        ul_TFCS:
                        [
                          normalTFCI_Signalling:
                          [
                            complete:
                            {
                              ctfcSize:
                              [
                                ctfc2Bit:
                                [
                                  {
                                    ctfc2: 0,
                                    powerOffsetInformation:
                                    {
                                      gainFactorInformation:
                                      [
                                        computedGainFactors: 0
                                      ],
                                      powerOffsetPp_m: OMIT
                                    }
                                  },

                                  {
                                    ctfc2: 1,
                                    powerOffsetInformation:
                                    {
                                      gainFactorInformation:
                                      [
                                        signalledGainFactors:
                                        {
                                          modeSpecificInfo:
                                          [
                                            fdd:
                                            {
                                              gainFactorBetaC: 11
                                            }
                                          ],
                                          gainFactorBetaD: 15,
                                          referenceTFC_ID: 0
                                        }
                                      ],
                                      powerOffsetPp_m: OMIT
                                    }
                                  }
                                ]
                              ]
                            }
                          ]
                        ]
                      }
                    ]
                  },
                  ul_AddReconfTransChInfoList:
                  [
                    {
                      ul_TransportChannelType: dch,
                      transportChannelIdentity: 5,
                      transportFormatSet:
                      [
                        dedicatedTransChTFS:
                        {
                          tti:
                          [
                            tti10:
                            [
                              {
                                rlc_Size:
                                [
                                  bitMode:
                                  [
                                    sizeType2:
                                    {
                                      part1: 2,
                                      part2: OMIT
                                    }
                                  ]
                                ],
                                numberOfTbSizeList:
                                [
                                  [
                                    zero: NULL
                                  ],

                                  [
                                    one: NULL
                                  ]
                                ],
                                logicalChannelList:
                                [
                                  allSizes: NULL
                                ]
                              }
                            ]
                          ],
                          semistaticTF_Information:
                          {
                            channelCodingType:
                            [
                              convolutional: third
                            ],
                            rateMatchingAttribute# 192 # crc_Size# crc16
                          }
                        }
                      ]
                    }
                  ]
                  # dl_CommonTransChInfo#
                  {
                    sccpch_TFCS# OMIT# modeSpecificInfo#
                    [
                      fdd#
                      {
                        dl_Parameters#
                        [
                          sameAsUL# NULL
                        ]
                      }
                    ]
                  }
                  # dl_AddReconfTransChInfoList#
                  [
                    {
                      dl_TransportChannelType# dch# dl_transportChannelIdentity# 10 # tfs_SignallingMode#
                      [
                        sameAsULTrCH#
                        {
                          ul_TransportChannelType# dch# ul_TransportChannelIdentity# 5
                        }
                      ]
                      # dch_QualityTarget#
                      {
                        bler_QualityValue# #20
                      }
                      # dummy# OMIT
                    }
                  ]
                  # frequencyInfo# OMIT# maxAllowedUL_TX_Power# OMIT# ul_ChannelRequirement#
                  [
                    ul_DPCH_Info#
                    {
                      ul_DPCH_PowerControlInfo#
                      [
                        fdd#
                        {
                          dpcch_PowerOffset# #40 # pc_Preamble# 1 # sRB_delay# 7 # powerControlAlgorithm#
                          [
                            algorithm1# 0
                          ]
                        }
                      ]
                      # modeSpecificInfo#
                      [
                        fdd#
                        {
                          scramblingCodeType# longSC# scramblingCode# 0 # numberOfDPDCH# OMIT# spreadingFactor# sf64# tfci_Existence# GcTRUE # numberOfFBI_Bits# OMIT# puncturingLimit# pl1
                        }
                      ]
                    }
                  ]
                  # dl_CommonInformation#
                  {
                    dl_DPCH_InfoCommon#
                    {
                      cfnHandling#
                      [
                        initialise#
                        {
                          cfntargetsfnframeoffset# OMIT
                        }
                      ]
                      # modeSpecificInfo#
                      [
                        fdd#
                        {
                          dl_DPCH_PowerControlInfo#
                          {
                            modeSpecificInfo#
                            [
                              fdd#
                              {
                                dpc_Mode# singleTPC
                              }
                            ]
                          }
                          # powerOffsetPilot_pdpdch# 0 # dl_rate_matching_restriction# OMIT# spreadingFactorAndPilot#
                          [
                            sfd128# pb4
                          ]
                          # positionFixedOrFlexible# fixed# tfci_Existence# GcFALSE
                        }
                      ]
                    }
                    # modeSpecificInfo#
                    [
                      fdd#
                      {
                        defaultDPCH_OffsetValue# 0 # dpch_CompressedModeInfo# OMIT# tx_DiversityMode# noDiversity# ssdt_Information# OMIT
                      }
                    ]
                  }
                  # dl_InformationPerRL_List#
                  [
                    {
                      modeSpecificInfo#
                      [
                        fdd#
                        {
                          primaryCPICH_Info#
                          {
                            primaryScramblingCode# 100
                          }
                          # pdsch_SHO_DCH_Info# OMIT# pdsch_CodeMapping# OMIT
                        }
                      ]
                      # dl_DPCH_InfoPerRL#
                      [
                        fdd#
                        {
                          pCPICH_UsageForChannelEst# mayBeUsed# dpch_FrameOffset# 0 # secondaryCPICH_Info# OMIT# dl_ChannelisationCodeList#
                          [
                            {
                              secondaryScramblingCode# 1 # sf_AndCodeNumber#
                              [
                                sf128# 0
                              ]
                              # scramblingCodeChange# noCodeChange
                            }
                          ]
                          # tpc_CombinationIndex# 0 # ssdt_CellIdentity# OMIT# closedLoopTimingAdjMode# OMIT
                        }
                      ]
                      # sccpch_InfoforFACH# OMIT
                    }
                  ]
                }
                # laterNonCriticalExtensions# OMIT
              }
            ]
          ]
        }
      ]
      # specialLI# GcTRUE
    }

TTCN PDU: RLC_AM_DATA_IND

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 2
      ],
      integrityResult:
      [
        integrityUsed: i_pass
      ],
      aM_message:
      [
        uL_DCCH_Message: PDU:
        {
          integrityCheckInfo: OMIT,
          message:
          [
            rrcConnectionSetupComplete:
            {
              rrc_TransactionIdentifier: 0,
              startList:
              [
                {
                  cn_DomainIdentity: ps_domain,
                  start_Value: '00000000000000000010'B
                },

                {
                  cn_DomainIdentity: cs_domain,
                  start_Value: '00000000000000000010'B
                }
              ],
              ue_RadioAccessCapability:
              {
                accessStratumReleaseIndicator: r99,
                pdcp_Capability:
                {
                  losslessSRNS_RelocationSupport: GcFALSE,
                  supportForRfc2507:
                  [
                    notSupported: NULL
                  ]
                },
                rlc_Capability:
                {
                  totalRLC_AM_BufferSize: kb50,
                  maximumRLC_WindowSize: mws2047,
                  maximumAM_EntityNumber: am6
                },
                transportChannelCapability:
                {
                  dl_TransChCapability:
                  {
                    maxNoBitsReceived: b8960,
                    maxConvCodeBitsReceived: b1280,
                    turboDecodingSupport:
                    [
                      supported: b8960
                    ],
                    maxSimultaneousTransChs: e8,
                    maxSimultaneousCCTrCH_Count: 1,
                    maxReceivedTransportBlocks: tb32,
                    maxNumberOfTFC: tfc128,
                    maxNumberOfTF: tf64
                  },
                  ul_TransChCapability:
                  {
                    maxNoBitsTransmitted: b3840,
                    maxConvCodeBitsTransmitted: b1280,
                    turboEncodingSupport:
                    [
                      supported: b3840
                    ],
                    maxSimultaneousTransChs: e8,
                    modeSpecificInfo:
                    [
                      fdd: NULL
                    ],
                    maxTransmittedBlocks: tb32,
                    maxNumberOfTFC: tfc64,
                    maxNumberOfTF: tf32
                  }
                },
                rf_Capability:
                {
                  fddRF_Capability:
                  {
                    ue_PowerClass: 4,
                    txRxFrequencySeparation: mhz190
                  },
                  tddRF_Capability: OMIT
                },
                physicalChannelCapability:
                {
                  fddPhysChCapability:
                  {
                    downlinkPhysChCapability:
                    {
                      maxNoDPCH_PDSCH_Codes: 1,
                      maxNoPhysChBitsReceived: b9600,
                      supportForSF_512: GcFALSE,
                      supportOfPDSCH: GcFALSE,
                      simultaneousSCCPCH_DPCH_Reception:
                      [
                        notSupported: NULL
                      ]
                    },
                    uplinkPhysChCapability:
                    {
                      maxNoDPDCH_BitsTransmitted: b4800,
                      supportOfPCPCH: GcFALSE
                    }
                  },
                  tddPhysChCapability: OMIT
                },
                ue_MultiModeRAT_Capability:
                {
                  multiRAT_CapabilityList:
                  {
                    supportOfGSM: GcFALSE,
                    supportOfMulticarrier: GcFALSE
                  },
                  multiModeCapability: fdd
                },
                securityCapability:
                {
                  cipheringAlgorithmCap: '0000000000000011'B,
                  integrityProtectionAlgorithmCap: '0000000000000010'B
                },
                ue_positioning_Capability:
                {
                  standaloneLocMethodsSupported: GcFALSE,
                  ue_BasedOTDOA_Supported: GcFALSE,
                  networkAssistedGPS_Supported: noNetworkAssistedGPS,
                  supportForUE_GPS_TimingOfCellFrames: GcFALSE,
                  supportForIPDL: GcFALSE
                },
                measurementCapability:
                {
                  downlinkCompressedMode:
                  {
                    fdd_Measurements: GcTRUE,
                    tdd_Measurements: OMIT,
                    gsm_Measurements:
                    {
                      gsm900: GcTRUE,
                      dcs1800: GcTRUE,
                      gsm1900: GcTRUE
                    },
                    multiCarrierMeasurements: GcFALSE
                  },
                  uplinkCompressedMode:
                  {
                    fdd_Measurements: GcTRUE,
                    tdd_Measurements: OMIT,
                    gsm_Measurements:
                    {
                      gsm900: GcTRUE,
                      dcs1800: GcTRUE,
                      gsm1900: GcTRUE
                    },
                    multiCarrierMeasurements: GcFALSE
                  }
                }
              },
              ue_RATSpecificCapability: OMIT,
              v370NonCriticalExtensions: OMIT
            }
          ]
        }
      ]
    }

TTCN PDU: RRC_DataInd

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      rB_Id: 3,
      ch: OMIT,
      sapId: OMIT,
      cN_Domain: 0,
      start: '00000000000000000010'B,
      msg: PDU:
      {
        skipIndicator: '0000'B,
        mMProtocolDiscriminator: '0101'B,
        msgType: '00001000'B,
        ciphKeySeqNum:
        {
          spare1: '0'B,
          keySeq: '111'B
        },
        locUpdType:
        {
          fOR: '0'B,
          spare1: '0'B,
          lUT: '00'B
        },
        locAreaId:
        {
          plmn: '00F110'O,
          lac: 'FFFE'O
        },
        mSClsmk1:
        {
          spare1: '0'B,
          revLvl: '10'B,
          eSIND: '0'B,
          a5_1: '1'B,
          rFPwrCap: '111'B
        },
        mobileId:
        {
          iel: '08'O,
          iDigit1: '0000'B,
          oddEvenInd: '1'B,
          typeOfId: '001'B,
          otherDigits: '10100000003033'O
        },
        mSClsmk2:
        {
          iei: '00110011'B,
          iel: '03'O,
          spare1_1: '0'B,
          revLvl: '10'B,
          eSIND: '0'B,
          a5_1: '1'B,
          rFPwrCap: '111'B,
          spare1_2: '0'B,
          pSCap: '0'B,
          sSSI: '01'B,
          sMCap: '1'B,
          vBS: '0'B,
          vGCS: '0'B,
          fC: '0'B,
          cM3: '1'B,
          spare1_3: '0'B,
          lCSVA: '1'B,
          uCS2: '0'B,
          soLSA: '0'B,
          cMSP: '0'B,
          a5_3: '0'B,
          a5_2: '0'B
        }
      }
    }

TTCN PDU: RRC_DataReq

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      rB_Id: 3,
      ch: OMIT,
      sapId: OMIT,
      cN_Domain: 0,
      msg: PDU:
      {
        skipIndicator: '0000'B,
        mMProtocolDiscriminator: '0101'B,
        msgType: '00010010'B,
        spare4: '0000'B,
        ciphKeySeqNum:
        {
          spare1: '0'B,
          keySeq: '000'B
        },
        rAND: '01010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101'B,
        aUTN:
        {
          iei: '00100000'B,
          iel: '10'O,
          aUTN: '01100110000100010000000000110011001000101101110100000000000000000101010101000100011101110110011000010001000000000011001100100010'B
        }
      }
    }

TTCN PDU: Assignment:[19] tcv_TmpAttachRe

(To search, click here and then press Ctrl+F)

    := PDU:
    {
      skipIndicator: '0000'B,
      gMMProtocolDiscriminator: '1000'B,
      msgType: '00000001'B,
      msNetworkCap:
      {
        iel: '02'O,
        value: 'E540'O
      },
      gprsCiphKeySeqNo:
      {
        spare1: '0'B,
        keySeq: '000'B
      },
      attachType:
      {
        for: '0'B,
        type: '001'B
      },
      drxParameter:
      {
        splitPGcycleCode: '00000111'B,
        cnDRXcoef: '0000'B,
        splitOnCCCH: '0'B,
        nonDRXtimer: '100'B
      },
      ptmsiORimsi:
      {
        iel: '05'O,
        iDigit1: '1111'B,
        oddEvenInd: '0'B,
        typeOfId: '100'B,
        otherDigits: '12345678'O
      },
      oldRAI:
      {
        plmn: '00F110'O,
        lac: '0002'O,
        rac: '05'O
      },
      msRadioAccessCap:
      {
        iel: '0B'O,
        value: '15F38233542A332644A198'O
      },
      oldPTMSI_Signature: OMIT,
      readyTimer:
      {
        iei: '00010111'B,
        unit: '000'B,
        value: '10110'B
      },
      tmsiStatus: OMIT
    }

TTCN PDU: RRC_DataInd

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      rB_Id: 3,
      ch: OMIT,
      sapId: OMIT,
      cN_Domain: 1,
      start: '00000000000000000010'B,
      msg: PDU:
      {
        skipIndicator: '0000'B,
        gMMProtocolDiscriminator: '1000'B,
        msgType: '00000001'B,
        msNetworkCap:
        {
          iel: '02'O,
          value: 'E540'O
        },
        gprsCiphKeySeqNo:
        {
          spare1: '0'B,
          keySeq: '000'B
        },
        attachType:
        {
          for: '0'B,
          type: '001'B
        },
        drxParameter:
        {
          splitPGcycleCode: '00000111'B,
          cnDRXcoef: '0000'B,
          splitOnCCCH: '0'B,
          nonDRXtimer: '100'B
        },
        ptmsiORimsi:
        {
          iel: '05'O,
          iDigit1: '1111'B,
          oddEvenInd: '0'B,
          typeOfId: '100'B,
          otherDigits: '12345678'O
        },
        oldRAI:
        {
          plmn: '00F110'O,
          lac: '0002'O,
          rac: '05'O
        },
        msRadioAccessCap:
        {
          iel: '0B'O,
          value: '15F38233542A332644A198'O
        },
        oldPTMSI_Signature: OMIT,
        readyTimer:
        {
          iei: '00010111'B,
          unit: '000'B,
          value: '10110'B
        },
        tmsiStatus: OMIT
      }
    }

TTCN PDU: Assignment:[3] tcv_AuthRs

(To search, click here and then press Ctrl+F)

    := PDU:
    {
      skipIndicator: '0000'B,
      mMProtocolDiscriminator: '0101'B,
      msgType: '01010100'B,
      authRsp: '01010101010001000111011101100110'B,
      authRspExt:
      {
        iei: '00100001'B,
        iel: '04'O,
        rES: '00010001000000000011001100100010'B
      }
    }

TTCN PDU: RRC_DataInd

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      rB_Id: 3,
      ch: OMIT,
      sapId: OMIT,
      cN_Domain: 0,
      start: OMIT,
      msg: PDU:
      {
        skipIndicator: '0000'B,
        mMProtocolDiscriminator: '0101'B,
        msgType: '01010100'B,
        authRsp: '01010101010001000111011101100110'B,
        authRspExt:
        {
          iei: '00100001'B,
          iel: '04'O,
          rES: '00010001000000000011001100100010'B
        }
      }
    }

TTCN PDU: CRLC_SecurityMode_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      rlcSecurityInfo:
      {
        cn_DomainIdentity: cs_domain,
        startValue: '00000000000000000000'B,
        cipheringKey: OMIT,
        integrityKey: '01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100'B,
        gsmCipheringKey: OMIT
      }
    }

TTCN PDU: CRLC_SetRRC_MessageSN_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: 0
      ],
      count_I_LSB_UL: OMIT,
      count_I_LSB_DL: 0
    }

TTCN PDU: CRLC_SetRRC_MessageSN_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 1
      ],
      count_I_LSB_UL: OMIT,
      count_I_LSB_DL: 0
    }

TTCN PDU: CRLC_SetRRC_MessageSN_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 2
      ],
      count_I_LSB_UL: OMIT,
      count_I_LSB_DL: 0
    }

TTCN PDU: CRLC_SetRRC_MessageSN_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 3
      ],
      count_I_LSB_UL: OMIT,
      count_I_LSB_DL: 0
    }

TTCN PDU: CRLC_SetRRC_MessageSN_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 4
      ],
      count_I_LSB_UL: OMIT,
      count_I_LSB_DL: 0
    }

TTCN PDU: CRLC_Integrity_Activate_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      cn_DomainIdentity: cs_domain,
      integrityActivationInfo:
      [
        integrityProtectionModeInfo:
        {
          integrityProtectionModeCommand:
          [
            startIntegrityProtection:
            {
              integrityProtInitNumber: '00001111000011110000111100001111'B
            }
          ],
          integrityProtectionAlgorithm: uia1
        }
      ]
    }

TTCN PDU: CRLC_Integrity_Activate_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      cn_DomainIdentity: cs_domain,
      integrityActivationInfo:
      [
        ul_IntegProtActivationInfo:
        [
          {
            rb_Identity: 2,
            rrc_MessageSequenceNumber: 0
          }
        ]
      ]
    }

TTCN PDU: RLC_AM_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 2
      ],
      confirmationRequest:
      [
        noConfirmationRequest: NULL
      ],
      aM_message:
      [
        dL_DCCH_Message: PDU:
        {
          integrityCheckInfo:
          {
            messageAuthenticationCode: '00010001001100011010010000011001'B,
            rrc_MessageSequenceNumber: 1
          },
          message:
          [
            securityModeCommand:
            [
              r3:
              {
                securityModeCommand_r3:
                {
                  rrc_TransactionIdentifier: 0,
                  securityCapability:
                  {
                    cipheringAlgorithmCap: '0000000000000011'B,
                    integrityProtectionAlgorithmCap: '0000000000000010'B
                  },
                  cipheringModeInfo: OMIT,
                  integrityProtectionModeInfo:
                  {
                    integrityProtectionModeCommand:
                    [
                      startIntegrityProtection:
                      {
                        integrityProtInitNumber: '00001111000011110000111100001111'B
                      }
                    ],
                    integrityProtectionAlgorithm: uia1
                  },
                  cn_DomainIdentity: cs_domain,
                  ue_SystemSpecificSecurityCap: OMIT
                },
                laterNonCriticalExtensions: OMIT
              }
            ]
          ]
        }
      ]
    }

TTCN PDU: RLC_AM_DATA_IND

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 2
      ],
      integrityResult:
      [
        integrityUsed: i_pass
      ],
      aM_message:
      [
        uL_DCCH_Message: PDU:
        {
          integrityCheckInfo:
          {
            messageAuthenticationCode: '10001011001000110111110011100010'B,
            rrc_MessageSequenceNumber: 1
          },
          message:
          [
            securityModeComplete:
            {
              rrc_TransactionIdentifier: 0,
              ul_IntegProtActivationInfo:
              {
                rrc_MessageSequenceNumberList:
                [
                  0,
                  0,
                  0,
                  0,
                  0
                ]
              },
              rb_UL_CiphActivationTimeInfo: OMIT,
              laterNonCriticalExtensions: OMIT
            }
          ]
        }
      ]
    }

TTCN PDU: CRLC_Integrity_Activate_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      cn_DomainIdentity: cs_domain,
      integrityActivationInfo:
      [
        ul_IntegProtActivationInfo:
        [
          {
            rb_Identity: 0,
            rrc_MessageSequenceNumber: 0
          },

          {
            rb_Identity: 1,
            rrc_MessageSequenceNumber: 0
          },

          {
            rb_Identity: 3,
            rrc_MessageSequenceNumber: 0
          },

          {
            rb_Identity: 4,
            rrc_MessageSequenceNumber: 0
          }
        ]
      ]
    }

TTCN PDU: RRC_DataReq

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      rB_Id: 3,
      ch: OMIT,
      sapId: OMIT,
      cN_Domain: 0,
      msg: PDU:
      {
        skipIndicator: '0000'B,
        mMProtocolDiscriminator: '0101'B,
        msgType: '00000010'B,
        locAreaId:
        {
          plmn: '00F110'O,
          lac: '0001'O
        },
        mobileId:
        {
          iei: '00010111'B,
          iel: '05'O,
          iDigit1: '1111'B,
          oddEvenInd: '0'B,
          typeOfId: '100'B,
          otherDigits: '11223344'O
        },
        followOnProceed: '10100001'B,
        cTSPerm: '10100010'B,
        equivalentPLMN: OMIT
      }
    }

TTCN PDU: RRC_DataInd

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      rB_Id: 3,
      ch: OMIT,
      sapId: OMIT,
      cN_Domain: 0,
      start: OMIT,
      msg: PDU:
      {
        skipIndicator: '0000'B,
        mMProtocolDiscriminator: '0101'B,
        msgType: '10011011'B
      }
    }

TTCN PDU: RRC_DataReq

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      rB_Id: 3,
      ch: OMIT,
      sapId: OMIT,
      cN_Domain: 1,
      msg: PDU:
      {
        skipIndicator: '0000'B,
        gMMProtocolDiscriminator: '1000'B,
        msgType: '00010010'B,
        imeisvReq:
        {
          spare1: '0'B,
          value: '000'B
        },
        ciphAlgorithm:
        {
          spare1: '0'B,
          algorithm: '001'B
        },
        acRefNo:
        {
          value: '0011'B
        },
        forceToStandby:
        {
          spare: '0'B,
          value: '000'B
        },
        authRand:
        {
          iei: '00100001'B,
          randValue: '01010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101'B
        },
        gprsCiphKeySeqNo:
        {
          iei: '1000'B,
          spare1: '0'B,
          keySeq: '000'B
        },
        aUTN:
        {
          iei: '00101000'B,
          iel: '10'O,
          aUTN: '01100110000100010000000000110011001000101101110100000000000000000101010101000100011101110110011000010001000000000011001100100010'B
        }
      }
    }

TTCN PDU: Assignment:[3] tcv_TmpAuthAndCiphRs

(To search, click here and then press Ctrl+F)

    := PDU:
    {
      skipIndicator: '0000'B,
      gMMProtocolDiscriminator: '1000'B,
      msgType: '00010011'B,
      spare4: '0000'B,
      acRefNo:
      {
        value: '0011'B
      },
      authRsp:
      {
        iei: '00100010'B,
        value: '01010101010001000111011101100110'B
      },
      imeisv: OMIT,
      authRspExt:
      {
        iei: '00101001'B,
        iel: '04'O,
        rES: '00010001000000000011001100100010'B
      }
    }

TTCN PDU: RRC_DataInd

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      rB_Id: 3,
      ch: OMIT,
      sapId: OMIT,
      cN_Domain: 1,
      start: OMIT,
      msg: PDU:
      {
        skipIndicator: '0000'B,
        gMMProtocolDiscriminator: '1000'B,
        msgType: '00010011'B,
        spare4: '0000'B,
        acRefNo:
        {
          value: '0011'B
        },
        authRsp:
        {
          iei: '00100010'B,
          value: '01010101010001000111011101100110'B
        },
        imeisv: OMIT,
        authRspExt:
        {
          iei: '00101001'B,
          iel: '04'O,
          rES: '00010001000000000011001100100010'B
        }
      }
    }

TTCN PDU: CRLC_RRC_MessageSN_CNF

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 0
      ],
      count_I_MSB_UL: 0,
      count_I_LSB_UL: 0,
      count_I_MSB_DL: 0,
      count_I_LSB_DL: 0
    }

TTCN PDU: CRLC_RRC_MessageSN_CNF

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 1
      ],
      count_I_MSB_UL: 0,
      count_I_LSB_UL: 0,
      count_I_MSB_DL: 0,
      count_I_LSB_DL: 0
    }

TTCN PDU: CRLC_RRC_MessageSN_CNF

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 2
      ],
      count_I_MSB_UL: 0,
      count_I_LSB_UL: 1,
      count_I_MSB_DL: 0,
      count_I_LSB_DL: 1
    }

TTCN PDU: CRLC_RRC_MessageSN_CNF

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 3
      ],
      count_I_MSB_UL: 0,
      count_I_LSB_UL: 2,
      count_I_MSB_DL: 0,
      count_I_LSB_DL: 2
    }

TTCN PDU: CRLC_RRC_MessageSN_CNF

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 4
      ],
      count_I_MSB_UL: 0,
      count_I_LSB_UL: 0,
      count_I_MSB_DL: 0,
      count_I_LSB_DL: 0
    }

TTCN PDU: CRLC_SecurityMode_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      rlcSecurityInfo:
      {
        cn_DomainIdentity: ps_domain,
        startValue: '00000000000000000000'B,
        cipheringKey: OMIT,
        integrityKey: '01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100'B,
        gsmCipheringKey: OMIT
      }
    }

TTCN PDU: CRLC_Integrity_Activate_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      cn_DomainIdentity: ps_domain,
      integrityActivationInfo:
      [
        integrityProtectionModeInfo:
        {
          integrityProtectionModeCommand:
          [
            modify:
            {
              dl_IntegrityProtActivationInfo:
              {
                rrc_MessageSequenceNumberList:
                [
                  0,
                  0,
                  1,
                  2,
                  0
                ]
              }
            }
          ],
          integrityProtectionAlgorithm: uia1
        }
      ]
    }

TTCN PDU: CRLC_Integrity_Activate_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      cn_DomainIdentity: ps_domain,
      integrityActivationInfo:
      [
        ul_IntegProtActivationInfo:
        [
          {
            rb_Identity: 2,
            rrc_MessageSequenceNumber: 1
          }
        ]
      ]
    }

TTCN PDU: RLC_AM_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 2
      ],
      confirmationRequest:
      [
        noConfirmationRequest: NULL
      ],
      aM_message:
      [
        dL_DCCH_Message: PDU:
        {
          integrityCheckInfo:
          {
            messageAuthenticationCode: '00100001110110000101111100011100'B,
            rrc_MessageSequenceNumber: 2
          },
          message:
          [
            securityModeCommand:
            [
              r3:
              {
                securityModeCommand_r3:
                {
                  rrc_TransactionIdentifier: 0,
                  securityCapability:
                  {
                    cipheringAlgorithmCap: '0000000000000011'B,
                    integrityProtectionAlgorithmCap: '0000000000000010'B
                  },
                  cipheringModeInfo: OMIT,
                  integrityProtectionModeInfo:
                  {
                    integrityProtectionModeCommand:
                    [
                      modify:
                      {
                        dl_IntegrityProtActivationInfo:
                        {
                          rrc_MessageSequenceNumberList:
                          [
                            0,
                            0,
                            1,
                            2,
                            0
                          ]
                        }
                      }
                    ],
                    integrityProtectionAlgorithm: uia1
                  },
                  cn_DomainIdentity: ps_domain,
                  ue_SystemSpecificSecurityCap: OMIT
                },
                laterNonCriticalExtensions: OMIT
              }
            ]
          ]
        }
      ]
    }

TTCN PDU: RLC_AM_DATA_IND

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 2
      ],
      integrityResult:
      [
        integrityUsed: i_pass
      ],
      aM_message:
      [
        uL_DCCH_Message: PDU:
        {
          integrityCheckInfo:
          {
            messageAuthenticationCode: '11100000000110011010110001001011'B,
            rrc_MessageSequenceNumber: 2
          },
          message:
          [
            securityModeComplete:
            {
              rrc_TransactionIdentifier: 0,
              ul_IntegProtActivationInfo:
              {
                rrc_MessageSequenceNumberList:
                [
                  5,
                  1,
                  2,
                  3,
                  1
                ]
              },
              rb_UL_CiphActivationTimeInfo: OMIT,
              laterNonCriticalExtensions: OMIT
            }
          ]
        }
      ]
    }

TTCN PDU: CRLC_Integrity_Activate_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      cn_DomainIdentity: ps_domain,
      integrityActivationInfo:
      [
        ul_IntegProtActivationInfo:
        [
          {
            rb_Identity: 0,
            rrc_MessageSequenceNumber: 5
          },

          {
            rb_Identity: 1,
            rrc_MessageSequenceNumber: 1
          },

          {
            rb_Identity: 3,
            rrc_MessageSequenceNumber: 3
          },

          {
            rb_Identity: 4,
            rrc_MessageSequenceNumber: 1
          }
        ]
      ]
    }

TTCN PDU: RRC_DataReq

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      rB_Id: 3,
      ch: OMIT,
      sapId: OMIT,
      cN_Domain: 1,
      msg: PDU:
      {
        skipIndicator: '0000'B,
        gMMProtocolDiscriminator: '1000'B,
        msgType: '00000010'B,
        forceToStandby:
        {
          spare: '0'B,
          value: '000'B
        },
        attachResult:
        {
          spare: '0'B,
          result: '001'B
        },
        periodicRAupdateTimer:
        {
          unit: '111'B,
          value: '00000'B
        },
        spare: '0000'B,
        radioPrioSMS:
        {
          spare: '0'B,
          value: '100'B
        },
        rai:
        {
          plmn: '00F110'O,
          lac: '0001'O,
          rac: '05'O
        },
        ptmsiSignature:
        {
          iei: '00011001'B,
          value: 'AB1234'O
        },
        negReadyTimer: OMIT,
        allocatedPTMSI:
        {
          iei: '00011000'B,
          iel: '05'O,
          iDigit1: '1111'B,
          oddEvenInd: '0'B,
          typeOfId: '100'B,
          otherDigits: '12345678'O
        },
        msIdentity: OMIT,
        gmmCause: OMIT,
        t3302Value: OMIT,
        cellNotification: OMIT,
        equivalentPLMN: OMIT
      }
    }

TTCN PDU: RRC_DataInd

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      rB_Id: 3,
      ch: OMIT,
      sapId: OMIT,
      cN_Domain: 1,
      start: OMIT,
      msg: PDU:
      {
        skipIndicator: '0000'B,
        gMMProtocolDiscriminator: '1000'B,
        msgType: '00000011'B
      }
    }

TTCN PDU: RLC_UM_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 1
      ],
      uM_message:
      [
        dL_DCCH_Message: PDU:
        {
          integrityCheckInfo:
          {
            messageAuthenticationCode: '11101100100111000001011111010011'B,
            rrc_MessageSequenceNumber: 1
          },
          message:
          [
            rrcConnectionRelease:
            [
              r3:
              {
                rrcConnectionRelease_r3:
                {
                  rrc_TransactionIdentifier: 0,
                  n_308: 1,
                  releaseCause: normalEvent,
                  rplmn_information: OMIT
                },
                laterNonCriticalExtensions: OMIT
              }
            ]
          ]
        }
      ],
      specialLI: GcFALSE
    }

TTCN PDU: RLC_UM_DATA_IND

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 1
      ],
      integrityResult:
      [
        integrityUsed: i_pass
      ],
      uM_message:
      [
        uL_DCCH_Message: PDU:
        {
          integrityCheckInfo:
          {
            messageAuthenticationCode: '11110111111000101100001011001110'B,
            rrc_MessageSequenceNumber: 1
          },
          message:
          [
            rrcConnectionReleaseComplete:
            {
              rrc_TransactionIdentifier: 0,
              errorIndication: OMIT,
              laterNonCriticalExtensions: OMIT
            }
          ]
        }
      ]
    }

TTCN PDU: RLC_UM_DATA_IND

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 1
      ],
      integrityResult:
      [
        integrityUsed: i_pass
      ],
      uM_message:
      [
        uL_DCCH_Message: PDU:
        {
          integrityCheckInfo:
          {
            messageAuthenticationCode: '10111001101000110000011111000000'B,
            rrc_MessageSequenceNumber: 2
          },
          message:
          [
            rrcConnectionReleaseComplete:
            {
              rrc_TransactionIdentifier: 0,
              errorIndication: OMIT,
              laterNonCriticalExtensions: OMIT
            }
          ]
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 1
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 2
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 3
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 4
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 1
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          sS_rlc_Info:
          {
            sS_ul_RLC_Mode:
            [
              dl_UM_RLC_Mode: NULL
            ],
            sS_dl_RLC_Mode:
            {
              dl_PayloadSize: 136,
              dl_RLCModeInfo:
              [
                ul_UM_RLC_Mode:
                {
                  transmissionRLC_Discard:
                  [
                    timerBasedNoExplicit: dt100
                  ]
                }
              ]
            }
          },
          rB_LogCH_Mapping:
          {
            uLlogicalChannelIdentity: 1,
            dLlogicalChannelIdentity: 1,
            logicalChannelType: OMIT,
            cn_DomainIdentity: OMIT
          }
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 2
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          sS_rlc_Info:
          {
            sS_ul_RLC_Mode:
            [
              dl_AM_RLC_Mode:
              {
                inSequenceDelivery: GcTRUE,
                receivingWindowSize: rw32,
                dl_RLC_StatusInfo:
                {
                  timerStatusProhibit: tsp200,
                  timerEPC: OMIT,
                  missingPDU_Indicator: GcTRUE,
                  timerStatusPeriodic: OMIT
                }
              }
            ],
            sS_dl_RLC_Mode:
            {
              dl_PayloadSize: 128,
              dl_RLCModeInfo:
              [
                ul_AM_RLC_Mode:
                {
                  transmissionRLC_Discard:
                  [
                    noDiscard: dat15
                  ],
                  transmissionWindowSize: tw32,
                  timerRST: tr500,
                  max_RST: rst1,
                  pollingInfo:
                  {
                    timerPollProhibit: tpp200,
                    timerPoll: tp200,
                    poll_PDU: OMIT,
                    poll_SDU: sdu1,
                    lastTransmissionPDU_Poll: GcTRUE,
                    lastRetransmissionPDU_Poll: GcTRUE,
                    pollWindow: pw99,
                    timerPollPeriodic: OMIT
                  }
                }
              ]
            }
          },
          rB_LogCH_Mapping:
          {
            uLlogicalChannelIdentity: 2,
            dLlogicalChannelIdentity: 2,
            logicalChannelType: OMIT,
            cn_DomainIdentity: OMIT
          }
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 3
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          sS_rlc_Info:
          {
            sS_ul_RLC_Mode:
            [
              dl_AM_RLC_Mode:
              {
                inSequenceDelivery: GcTRUE,
                receivingWindowSize: rw32,
                dl_RLC_StatusInfo:
                {
                  timerStatusProhibit: tsp200,
                  timerEPC: OMIT,
                  missingPDU_Indicator: GcTRUE,
                  timerStatusPeriodic: OMIT
                }
              }
            ],
            sS_dl_RLC_Mode:
            {
              dl_PayloadSize: 128,
              dl_RLCModeInfo:
              [
                ul_AM_RLC_Mode:
                {
                  transmissionRLC_Discard:
                  [
                    noDiscard: dat15
                  ],
                  transmissionWindowSize: tw32,
                  timerRST: tr500,
                  max_RST: rst1,
                  pollingInfo:
                  {
                    timerPollProhibit: tpp200,
                    timerPoll: tp200,
                    poll_PDU: OMIT,
                    poll_SDU: sdu1,
                    lastTransmissionPDU_Poll: GcTRUE,
                    lastRetransmissionPDU_Poll: GcTRUE,
                    pollWindow: pw99,
                    timerPollPeriodic: OMIT
                  }
                }
              ]
            }
          },
          rB_LogCH_Mapping:
          {
            uLlogicalChannelIdentity: 3,
            dLlogicalChannelIdentity: 3,
            logicalChannelType: OMIT,
            cn_DomainIdentity: OMIT
          }
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 4
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          sS_rlc_Info:
          {
            sS_ul_RLC_Mode:
            [
              dl_AM_RLC_Mode:
              {
                inSequenceDelivery: GcTRUE,
                receivingWindowSize: rw32,
                dl_RLC_StatusInfo:
                {
                  timerStatusProhibit: tsp200,
                  timerEPC: OMIT,
                  missingPDU_Indicator: GcTRUE,
                  timerStatusPeriodic: OMIT
                }
              }
            ],
            sS_dl_RLC_Mode:
            {
              dl_PayloadSize: 128,
              dl_RLCModeInfo:
              [
                ul_AM_RLC_Mode:
                {
                  transmissionRLC_Discard:
                  [
                    noDiscard: dat15
                  ],
                  transmissionWindowSize: tw32,
                  timerRST: tr500,
                  max_RST: rst1,
                  pollingInfo:
                  {
                    timerPollProhibit: tpp200,
                    timerPoll: tp200,
                    poll_PDU: OMIT,
                    poll_SDU: sdu1,
                    lastTransmissionPDU_Poll: GcTRUE,
                    lastRetransmissionPDU_Poll: GcTRUE,
                    pollWindow: pw99,
                    timerPollPeriodic: OMIT
                  }
                }
              ]
            }
          },
          rB_LogCH_Mapping:
          {
            uLlogicalChannelIdentity: 4,
            dLlogicalChannelIdentity: 4,
            logicalChannelType: OMIT,
            cn_DomainIdentity: OMIT
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 11,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              completeSIB_List:
              [
                {
                  sib_Type: systemInformationBlockType1,
                  sib_Data_variable: '1100010000000000000001011000100000101000000010100001000000000000000001000000000000000000000011000111010000'B
                },

                {
                  sib_Type: systemInformationBlockType2,
                  sib_Data_variable: '00000000000000000001'B
                }
              ]
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 3,
        sg_POS: 0,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              completeSIB_List:
              [
                {
                  sib_Type: masterInformationBlock,
                  sib_Data_variable: '0010000000000000010000000010010110101100000100010000000000011000100010110000110000100010110001010000100010100001110000100110100010010110010010010011000100010000'B
                }
              ]
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_PAGING_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 5
      ],
      ratType: fdd,
      configMessage:
      {
        pI_BitMapInfo:
        [
          e18: '000000000000000100'B
        ],
        dRX_CycleLength: 7,
        iMSI:
        [
          0,
          0,
          1,
          0,
          1,
          0,
          0,
          0,
          0,
          0,
          0,
          0,
          3,
          3,
          3
        ],
        t_pich_T_sccpch: GcFALSE
      }
    }

TTCN PDU: CMAC_PAGING_Config_CNF

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 5
      ]
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -2
      ],
      tM_message:
      [
        pCCH_Message: PDU:
        {
          message:
          [
            pagingType1:
            {
              pagingRecordList: OMIT,
              bcch_ModificationInfo:
              {
                mib_ValueTag: 3,
                bcch_ModificationTime: OMIT
              },
              laterNonCriticalExtensions: OMIT
            }
          ]
        }
      ]
    }

TTCN PDU: RLC_TR_DATA_IND

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: 0
      ],
      tM_message:
      [
        uL_CCCH_Message: PDU:
        {
          integrityCheckInfo: OMIT,
          message:
          [
            rrcConnectionRequest:
            {
              initialUE_Identity:
              [
                tmsi_and_LAI:
                {
                  tmsi: '00010001001000100011001101000100'B,
                  lai:
                  {
                    plmn_Identity:
                    {
                      mcc:
                      [
                        0,
                        0,
                        1
                      ],
                      mnc:
                      [
                        0,
                        1
                      ]
                    },
                    lac: '0000000000000001'B
                  }
                }
              ],
              establishmentCause: detach,
              protocolErrorIndicator: noError,
              measuredResultsOnRACH: OMIT,
              v3d0NonCriticalExtensions: OMIT
            }
          ]
        }
      ]
    }

TTCN PDU: RLC_UM_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: 0
      ],
      uM_message:
      [
        dL_CCCH_Message: PDU:
        {
          integrityCheckInfo: OMIT,
          message:
          [
            rrcConnectionSetup:
            [
              r3:
              {
                rrcConnectionSetup_r3:
                {
                  initialUE_Identity:
                  [
                    tmsi_and_LAI:
                    {
                      tmsi: '00010001001000100011001101000100'B,
                      lai:
                      {
                        plmn_Identity:
                        {
                          mcc:
                          [
                            0,
                            0,
                            1
                          ],
                          mnc:
                          [
                            0,
                            1
                          ]
                        },
                        lac: '0000000000000001'B
                      }
                    }
                  ],
                  rrc_TransactionIdentifier: 0,
                  activationTime: OMIT,
                  new_U_RNTI:
                  {
                    srnc_Identity: '000000000001'B,
                    s_RNTI: '00000000000000000001'B
                  },
                  new_c_RNTI: OMIT,
                  rrc_StateIndicator: cell_DCH,
                  utran_DRX_CycleLengthCoeff: 9,
                  capabilityUpdateRequirement:
                  {
                    ue_RadioCapabilityFDDUpdateRequirement: GcTRUE,
                    ue_RadioCapabilityTDDUpdateRequirement: GcFALSE,
                    systemSpecificCapUpdateReqList:
                    [
                      gsm
                    ]
                  },
                  srb_InformationSetupList:
                  [
                    {
                      rb_Identity: OMIT,
                      rlc_InfoChoice:
                      [
                        rlc_Info:
                        {
                          ul_RLC_Mode:
                          [
                            ul_UM_RLC_Mode:
                            {
                              transmissionRLC_Discard: OMIT
                            }
                          ],
                          dl_RLC_Mode:
                          [
                            dl_UM_RLC_Mode: NULL
                          ]
                        }
                      ],
                      rb_MappingInfo:
                      [
                        {
                          ul_LogicalChannelMappings:
                          [
                            oneLogicalChannel:
                            {
                              ul_TransportChannelType:
                              [
                                dch: 5
                              ],
                              logicalChannelIdentity: 1,
                              rlc_SizeList:
                              [
                                configured: NULL
                              ],
                              mac_LogicalChannelPriority: 1
                            }
                          ],
                          dl_LogicalChannelMappingList:
                          [
                            {
                              dl_TransportChannelType:
                              [
                                dch: 10
                              ],
                              logicalChannelIdentity: 1
                            }
                          ]
                        },

                        {
                          ul_LogicalChannelMappings:
                          [
                            oneLogicalChannel:
                            {
                              ul_TransportChannelType:
                              [
                                rach: NULL
                              ],
                              logicalChannelIdentity: 1,
                              rlc_SizeList:
                              [
                                explicitList:
                                [
                                  {
                                    rlc_SizeIndex: 1
                                  }
                                ]
                              ],
                              mac_LogicalChannelPriority: 1
                            }
                          ],
                          dl_LogicalChannelMappingList:
                          [
                            {
                              dl_TransportChannelType:
                              [
                                fach: NULL
                              ],
                              logicalChannelIdentity: 1
                            }
                          ]
                        }
                      ]
                    },

                    {
                      rb_Identity: OMIT,
                      rlc_InfoChoice:
                      [
                        rlc_Info:
                        {
                          ul_RLC_Mode:
                          [
                            ul_AM_RLC_Mode:
                            {
                              transmissionRLC_Discard:
                              [
                                noDiscard: dat15
                              ],
                              transmissionWindowSize: tw32,
                              timerRST: tr500,
                              max_RST: rst1,
                              pollingInfo:
                              {
                                timerPollProhibit: tpp200,
                                timerPoll: tp200,
                                poll_PDU: OMIT,
                                poll_SDU: sdu1,
                                lastTransmissionPDU_Poll: GcTRUE,
                                lastRetransmissionPDU_Poll: GcTRUE,
                                pollWindow: pw99,
                                timerPollPeriodic: OMIT
                              }
                            }
                          ],
                          dl_RLC_Mode:
                          [
                            dl_AM_RLC_Mode:
                            {
                              inSequenceDelivery: GcTRUE,
                              receivingWindowSize: rw32,
                              dl_RLC_StatusInfo:
                              {
                                timerStatusProhibit: tsp200,
                                timerEPC: OMIT,
                                missingPDU_Indicator: GcTRUE,
                                timerStatusPeriodic: OMIT
                              }
                            }
                          ]
                        }
                      ],
                      rb_MappingInfo:
                      [
                        {
                          ul_LogicalChannelMappings:
                          [
                            oneLogicalChannel:
                            {
                              ul_TransportChannelType:
                              [
                                dch: 5
                              ],
                              logicalChannelIdentity: 2,
                              rlc_SizeList:
                              [
                                configured: NULL
                              ],
                              mac_LogicalChannelPriority: 2
                            }
                          ],
                          dl_LogicalChannelMappingList:
                          [
                            {
                              dl_TransportChannelType:
                              [
                                dch: 10
                              ],
                              logicalChannelIdentity: 2
                            }
                          ]
                        },

                        {
                          ul_LogicalChannelMappings:
                          [
                            oneLogicalChannel:
                            {
                              ul_TransportChannelType:
                              [
                                rach: NULL
                              ],
                              logicalChannelIdentity: 2,
                              rlc_SizeList:
                              [
                                explicitList:
                                [
                                  {
                                    rlc_SizeIndex: 1
                                  }
                                ]
                              ],
                              mac_LogicalChannelPriority: 2
                            }
                          ],
                          dl_LogicalChannelMappingList:
                          [
                            {
                              dl_TransportChannelType:
                              [
                                fach: NULL
                              ],
                              logicalChannelIdentity: 2
                            }
                          ]
                        }
                      ]
                    },

                    {
                      rb_Identity: OMIT,
                      rlc_InfoChoice:
                      [
                        rlc_Info:
                        {
                          ul_RLC_Mode:
                          [
                            ul_AM_RLC_Mode:
                            {
                              transmissionRLC_Discard:
                              [
                                noDiscard: dat15
                              ],
                              transmissionWindowSize: tw32,
                              timerRST: tr500,
                              max_RST: rst1,
                              pollingInfo:
                              {
                                timerPollProhibit: tpp200,
                                timerPoll: tp200,
                                poll_PDU: OMIT,
                                poll_SDU: sdu1,
                                lastTransmissionPDU_Poll: GcTRUE,
                                lastRetransmissionPDU_Poll: GcTRUE,
                                pollWindow: pw99,
                                timerPollPeriodic: OMIT
                              }
                            }
                          ],
                          dl_RLC_Mode:
                          [
                            dl_AM_RLC_Mode:
                            {
                              inSequenceDelivery: GcTRUE,
                              receivingWindowSize: rw32,
                              dl_RLC_StatusInfo:
                              {
                                timerStatusProhibit: tsp200,
                                timerEPC: OMIT,
                                missingPDU_Indicator: GcTRUE,
                                timerStatusPeriodic: OMIT
                              }
                            }
                          ]
                        }
                      ],
                      rb_MappingInfo:
                      [
                        {
                          ul_LogicalChannelMappings:
                          [
                            oneLogicalChannel:
                            {
                              ul_TransportChannelType:
                              [
                                dch: 5
                              ],
                              logicalChannelIdentity: 3,
                              rlc_SizeList:
                              [
                                configured: NULL
                              ],
                              mac_LogicalChannelPriority: 3
                            }
                          ],
                          dl_LogicalChannelMappingList:
                          [
                            {
                              dl_TransportChannelType:
                              [
                                dch: 10
                              ],
                              logicalChannelIdentity: 3
                            }
                          ]
                        },

                        {
                          ul_LogicalChannelMappings:
                          [
                            oneLogicalChannel:
                            {
                              ul_TransportChannelType:
                              [
                                rach: NULL
                              ],
                              logicalChannelIdentity: 3,
                              rlc_SizeList:
                              [
                                explicitList:
                                [
                                  {
                                    rlc_SizeIndex: 1
                                  }
                                ]
                              ],
                              mac_LogicalChannelPriority: 3
                            }
                          ],
                          dl_LogicalChannelMappingList:
                          [
                            {
                              dl_TransportChannelType:
                              [
                                fach: NULL
                              ],
                              logicalChannelIdentity: 3
                            }
                          ]
                        }
                      ]
                    },

                    {
                      rb_Identity: OMIT,
                      rlc_InfoChoice:
                      [
                        rlc_Info:
                        {
                          ul_RLC_Mode:
                          [
                            ul_AM_RLC_Mode:
                            {
                              transmissionRLC_Discard:
                              [
                                noDiscard: dat15
                              ],
                              transmissionWindowSize: tw32,
                              timerRST: tr500,
                              max_RST: rst1,
                              pollingInfo:
                              {
                                timerPollProhibit: tpp200,
                                timerPoll: tp200,
                                poll_PDU: OMIT,
                                poll_SDU: sdu1,
                                lastTransmissionPDU_Poll: GcTRUE,
                                lastRetransmissionPDU_Poll: GcTRUE,
                                pollWindow: pw99,
                                timerPollPeriodic: OMIT
                              }
                            }
                          ],
                          dl_RLC_Mode:
                          [
                            dl_AM_RLC_Mode:
                            {
                              inSequenceDelivery: GcTRUE,
                              receivingWindowSize: rw32,
                              dl_RLC_StatusInfo:
                              {
                                timerStatusProhibit: tsp200,
                                timerEPC: OMIT,
                                missingPDU_Indicator: GcTRUE,
                                timerStatusPeriodic: OMIT
                              }
                            }
                          ]
                        }
                      ],
                      rb_MappingInfo:
                      [
                        {
                          ul_LogicalChannelMappings:
                          [
                            oneLogicalChannel:
                            {
                              ul_TransportChannelType:
                              [
                                dch: 5
                              ],
                              logicalChannelIdentity: 4,
                              rlc_SizeList:
                              [
                                configured: NULL
                              ],
                              mac_LogicalChannelPriority: 4
                            }
                          ],
                          dl_LogicalChannelMappingList:
                          [
                            {
                              dl_TransportChannelType:
                              [
                                dch: 10
                              ],
                              logicalChannelIdentity: 4
                            }
                          ]
                        },

                        {
                          ul_LogicalChannelMappings:
                          [
                            oneLogicalChannel:
                            {
                              ul_TransportChannelType:
                              [
                                rach: NULL
                              ],
                              logicalChannelIdentity: 4,
                              rlc_SizeList:
                              [
                                explicitList:
                                [
                                  {
                                    rlc_SizeIndex: 1
                                  }
                                ]
                              ],
                              mac_LogicalChannelPriority: 4
                            }
                          ],
                          dl_LogicalChannelMappingList:
                          [
                            {
                              dl_TransportChannelType:
                              [
                                fach: NULL
                              ],
                              logicalChannelIdentity: 4
                            }
                          ]
                        }
                      ]
                    }
                  ],
                  ul_CommonTransChInfo:
                  {
                    tfc_Subset: OMIT,
                    prach_TFCS: OMIT,
                    modeSpecificInfo:
                    [
                      fdd:
                      {
                        ul_TFCS:
                        [
                          normalTFCI_Signalling:
                          [
                            complete:
                            {
                              ctfcSize:
                              [
                                ctfc2Bit:
                                [
                                  {
                                    ctfc2: 0,
                                    powerOffsetInformation:
                                    {
                                      gainFactorInformation:
                                      [
                                        computedGainFactors: 0
                                      ],
                                      powerOffsetPp_m: OMIT
                                    }
                                  },

                                  {
                                    ctfc2: 1,
                                    powerOffsetInformation:
                                    {
                                      gainFactorInformation:
                                      [
                                        signalledGainFactors:
                                        {
                                          modeSpecificInfo:
                                          [
                                            fdd:
                                            {
                                              gainFactorBetaC: 11
                                            }
                                          ],
                                          gainFactorBetaD: 15,
                                          referenceTFC_ID: 0
                                        }
                                      ],
                                      powerOffsetPp_m: OMIT
                                    }
                                  }
                                ]
                              ]
                            }
                          ]
                        ]
                      }
                    ]
                  },
                  ul_AddReconfTransChInfoList:
                  [
                    {
                      ul_TransportChannelType: dch,
                      transportChannelIdentity: 5,
                      transportFormatSet:
                      [
                        dedicatedTransChTFS:
                        {
                          tti:
                          [
                            tti10:
                            [
                              {
                                rlc_Size:
                                [
                                  bitMode:
                                  [
                                    sizeType2:
                                    {
                                      part1: 2,
                                      part2: OMIT
                                    }
                                  ]
                                ],
                                numberOfTbSizeList:
                                [
                                  [
                                    zero: NULL
                                  ],

                                  [
                                    one: NULL
                                  ]
                                ],
                                logicalChannelList:
                                [
                                  allSizes: NULL
                                ]
                              }
                            ]
                          ],
                          semistaticTF_Information:
                          {
                            channelCodingType:
                            [
                              convolutional: third
                            ],
                            rateMatchingAttribute# 192 # crc_Size# crc16
                          }
                        }
                      ]
                    }
                  ]
                  # dl_CommonTransChInfo#
                  {
                    sccpch_TFCS# OMIT# modeSpecificInfo#
                    [
                      fdd#
                      {
                        dl_Parameters#
                        [
                          sameAsUL# NULL
                        ]
                      }
                    ]
                  }
                  # dl_AddReconfTransChInfoList#
                  [
                    {
                      dl_TransportChannelType# dch# dl_transportChannelIdentity# 10 # tfs_SignallingMode#
                      [
                        sameAsULTrCH#
                        {
                          ul_TransportChannelType# dch# ul_TransportChannelIdentity# 5
                        }
                      ]
                      # dch_QualityTarget#
                      {
                        bler_QualityValue# #20
                      }
                      # dummy# OMIT
                    }
                  ]
                  # frequencyInfo# OMIT# maxAllowedUL_TX_Power# OMIT# ul_ChannelRequirement#
                  [
                    ul_DPCH_Info#
                    {
                      ul_DPCH_PowerControlInfo#
                      [
                        fdd#
                        {
                          dpcch_PowerOffset# #40 # pc_Preamble# 1 # sRB_delay# 7 # powerControlAlgorithm#
                          [
                            algorithm1# 0
                          ]
                        }
                      ]
                      # modeSpecificInfo#
                      [
                        fdd#
                        {
                          scramblingCodeType# longSC# scramblingCode# 0 # numberOfDPDCH# OMIT# spreadingFactor# sf64# tfci_Existence# GcTRUE # numberOfFBI_Bits# OMIT# puncturingLimit# pl1
                        }
                      ]
                    }
                  ]
                  # dl_CommonInformation#
                  {
                    dl_DPCH_InfoCommon#
                    {
                      cfnHandling#
                      [
                        initialise#
                        {
                          cfntargetsfnframeoffset# OMIT
                        }
                      ]
                      # modeSpecificInfo#
                      [
                        fdd#
                        {
                          dl_DPCH_PowerControlInfo#
                          {
                            modeSpecificInfo#
                            [
                              fdd#
                              {
                                dpc_Mode# singleTPC
                              }
                            ]
                          }
                          # powerOffsetPilot_pdpdch# 0 # dl_rate_matching_restriction# OMIT# spreadingFactorAndPilot#
                          [
                            sfd128# pb4
                          ]
                          # positionFixedOrFlexible# fixed# tfci_Existence# GcFALSE
                        }
                      ]
                    }
                    # modeSpecificInfo#
                    [
                      fdd#
                      {
                        defaultDPCH_OffsetValue# 0 # dpch_CompressedModeInfo# OMIT# tx_DiversityMode# noDiversity# ssdt_Information# OMIT
                      }
                    ]
                  }
                  # dl_InformationPerRL_List#
                  [
                    {
                      modeSpecificInfo#
                      [
                        fdd#
                        {
                          primaryCPICH_Info#
                          {
                            primaryScramblingCode# 100
                          }
                          # pdsch_SHO_DCH_Info# OMIT# pdsch_CodeMapping# OMIT
                        }
                      ]
                      # dl_DPCH_InfoPerRL#
                      [
                        fdd#
                        {
                          pCPICH_UsageForChannelEst# mayBeUsed# dpch_FrameOffset# 0 # secondaryCPICH_Info# OMIT# dl_ChannelisationCodeList#
                          [
                            {
                              secondaryScramblingCode# 1 # sf_AndCodeNumber#
                              [
                                sf128# 0
                              ]
                              # scramblingCodeChange# noCodeChange
                            }
                          ]
                          # tpc_CombinationIndex# 0 # ssdt_CellIdentity# OMIT# closedLoopTimingAdjMode# OMIT
                        }
                      ]
                      # sccpch_InfoforFACH# OMIT
                    }
                  ]
                }
                # laterNonCriticalExtensions# OMIT
              }
            ]
          ]
        }
      ]
      # specialLI# GcTRUE
    }

TTCN PDU: RLC_AM_DATA_IND

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 2
      ],
      integrityResult:
      [
        integrityUsed: i_pass
      ],
      aM_message:
      [
        uL_DCCH_Message: PDU:
        {
          integrityCheckInfo: OMIT,
          message:
          [
            rrcConnectionSetupComplete:
            {
              rrc_TransactionIdentifier: 0,
              startList:
              [
                {
                  cn_DomainIdentity: ps_domain,
                  start_Value: '00000000000000000010'B
                },

                {
                  cn_DomainIdentity: cs_domain,
                  start_Value: '00000000000000000010'B
                }
              ],
              ue_RadioAccessCapability:
              {
                accessStratumReleaseIndicator: r99,
                pdcp_Capability:
                {
                  losslessSRNS_RelocationSupport: GcFALSE,
                  supportForRfc2507:
                  [
                    notSupported: NULL
                  ]
                },
                rlc_Capability:
                {
                  totalRLC_AM_BufferSize: kb50,
                  maximumRLC_WindowSize: mws2047,
                  maximumAM_EntityNumber: am6
                },
                transportChannelCapability:
                {
                  dl_TransChCapability:
                  {
                    maxNoBitsReceived: b8960,
                    maxConvCodeBitsReceived: b1280,
                    turboDecodingSupport:
                    [
                      supported: b8960
                    ],
                    maxSimultaneousTransChs: e8,
                    maxSimultaneousCCTrCH_Count: 1,
                    maxReceivedTransportBlocks: tb32,
                    maxNumberOfTFC: tfc128,
                    maxNumberOfTF: tf64
                  },
                  ul_TransChCapability:
                  {
                    maxNoBitsTransmitted: b3840,
                    maxConvCodeBitsTransmitted: b1280,
                    turboEncodingSupport:
                    [
                      supported: b3840
                    ],
                    maxSimultaneousTransChs: e8,
                    modeSpecificInfo:
                    [
                      fdd: NULL
                    ],
                    maxTransmittedBlocks: tb32,
                    maxNumberOfTFC: tfc64,
                    maxNumberOfTF: tf32
                  }
                },
                rf_Capability:
                {
                  fddRF_Capability:
                  {
                    ue_PowerClass: 4,
                    txRxFrequencySeparation: mhz190
                  },
                  tddRF_Capability: OMIT
                },
                physicalChannelCapability:
                {
                  fddPhysChCapability:
                  {
                    downlinkPhysChCapability:
                    {
                      maxNoDPCH_PDSCH_Codes: 1,
                      maxNoPhysChBitsReceived: b9600,
                      supportForSF_512: GcFALSE,
                      supportOfPDSCH: GcFALSE,
                      simultaneousSCCPCH_DPCH_Reception:
                      [
                        notSupported: NULL
                      ]
                    },
                    uplinkPhysChCapability:
                    {
                      maxNoDPDCH_BitsTransmitted: b4800,
                      supportOfPCPCH: GcFALSE
                    }
                  },
                  tddPhysChCapability: OMIT
                },
                ue_MultiModeRAT_Capability:
                {
                  multiRAT_CapabilityList:
                  {
                    supportOfGSM: GcFALSE,
                    supportOfMulticarrier: GcFALSE
                  },
                  multiModeCapability: fdd
                },
                securityCapability:
                {
                  cipheringAlgorithmCap: '0000000000000011'B,
                  integrityProtectionAlgorithmCap: '0000000000000010'B
                },
                ue_positioning_Capability:
                {
                  standaloneLocMethodsSupported: GcFALSE,
                  ue_BasedOTDOA_Supported: GcFALSE,
                  networkAssistedGPS_Supported: noNetworkAssistedGPS,
                  supportForUE_GPS_TimingOfCellFrames: GcFALSE,
                  supportForIPDL: GcFALSE
                },
                measurementCapability:
                {
                  downlinkCompressedMode:
                  {
                    fdd_Measurements: GcTRUE,
                    tdd_Measurements: OMIT,
                    gsm_Measurements:
                    {
                      gsm900: GcTRUE,
                      dcs1800: GcTRUE,
                      gsm1900: GcTRUE
                    },
                    multiCarrierMeasurements: GcFALSE
                  },
                  uplinkCompressedMode:
                  {
                    fdd_Measurements: GcTRUE,
                    tdd_Measurements: OMIT,
                    gsm_Measurements:
                    {
                      gsm900: GcTRUE,
                      dcs1800: GcTRUE,
                      gsm1900: GcTRUE
                    },
                    multiCarrierMeasurements: GcFALSE
                  }
                }
              },
              ue_RATSpecificCapability: OMIT,
              v370NonCriticalExtensions: OMIT
            }
          ]
        }
      ]
    }

TTCN PDU: RRC_DataInd

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      rB_Id: 3,
      ch: OMIT,
      sapId: OMIT,
      cN_Domain: 1,
      start: '00000000000000000010'B,
      msg: PDU:
      {
        skipIndicator: '0000'B,
        gMMProtocolDiscriminator: '1000'B,
        msgType: '00000101'B,
        spare4: '0000'B,
        detachType:
        {
          powOff: '1'B,
          type: '001'B
        },
        ptmsi:
        {
          iei: '00011000'B,
          iel: '05'O,
          iDigit1: '1111'B,
          oddEvenInd: '0'B,
          typeOfId: '100'B,
          otherDigits: '12345678'O
        },
        ptmsiSignature:
        {
          iei: '00011001'B,
          iel: '03'O,
          value: 'AB1234'O
        }
      }
    }

TTCN PDU: RLC_UM_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 1
      ],
      uM_message:
      [
        dL_DCCH_Message: PDU:
        {
          integrityCheckInfo: OMIT,
          message:
          [
            rrcConnectionRelease:
            [
              r3:
              {
                rrcConnectionRelease_r3:
                {
                  rrc_TransactionIdentifier: 0,
                  n_308: 1,
                  releaseCause: normalEvent,
                  rplmn_information: OMIT
                },
                laterNonCriticalExtensions: OMIT
              }
            ]
          ]
        }
      ],
      specialLI: GcFALSE
    }

TTCN PDU: RLC_UM_DATA_IND

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 1
      ],
      integrityResult:
      [
        integrityUsed: i_pass
      ],
      uM_message:
      [
        uL_DCCH_Message: PDU:
        {
          integrityCheckInfo: OMIT,
          message:
          [
            rrcConnectionReleaseComplete:
            {
              rrc_TransactionIdentifier: 0,
              errorIndication: OMIT,
              laterNonCriticalExtensions: OMIT
            }
          ]
        }
      ]
    }

TTCN PDU: RLC_UM_DATA_IND

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 1
      ],
      integrityResult:
      [
        integrityUsed: i_pass
      ],
      uM_message:
      [
        uL_DCCH_Message: PDU:
        {
          integrityCheckInfo: OMIT,
          message:
          [
            rrcConnectionReleaseComplete:
            {
              rrc_TransactionIdentifier: 0,
              errorIndication: OMIT,
              laterNonCriticalExtensions: OMIT
            }
          ]
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 1
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 2
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 3
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 4
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 1
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          sS_rlc_Info:
          {
            sS_ul_RLC_Mode:
            [
              dl_UM_RLC_Mode: NULL
            ],
            sS_dl_RLC_Mode:
            {
              dl_PayloadSize: 136,
              dl_RLCModeInfo:
              [
                ul_UM_RLC_Mode:
                {
                  transmissionRLC_Discard:
                  [
                    timerBasedNoExplicit: dt100
                  ]
                }
              ]
            }
          },
          rB_LogCH_Mapping:
          {
            uLlogicalChannelIdentity: 1,
            dLlogicalChannelIdentity: 1,
            logicalChannelType: OMIT,
            cn_DomainIdentity: OMIT
          }
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 2
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          sS_rlc_Info:
          {
            sS_ul_RLC_Mode:
            [
              dl_AM_RLC_Mode:
              {
                inSequenceDelivery: GcTRUE,
                receivingWindowSize: rw32,
                dl_RLC_StatusInfo:
                {
                  timerStatusProhibit: tsp200,
                  timerEPC: OMIT,
                  missingPDU_Indicator: GcTRUE,
                  timerStatusPeriodic: OMIT
                }
              }
            ],
            sS_dl_RLC_Mode:
            {
              dl_PayloadSize: 128,
              dl_RLCModeInfo:
              [
                ul_AM_RLC_Mode:
                {
                  transmissionRLC_Discard:
                  [
                    noDiscard: dat15
                  ],
                  transmissionWindowSize: tw32,
                  timerRST: tr500,
                  max_RST: rst1,
                  pollingInfo:
                  {
                    timerPollProhibit: tpp200,
                    timerPoll: tp200,
                    poll_PDU: OMIT,
                    poll_SDU: sdu1,
                    lastTransmissionPDU_Poll: GcTRUE,
                    lastRetransmissionPDU_Poll: GcTRUE,
                    pollWindow: pw99,
                    timerPollPeriodic: OMIT
                  }
                }
              ]
            }
          },
          rB_LogCH_Mapping:
          {
            uLlogicalChannelIdentity: 2,
            dLlogicalChannelIdentity: 2,
            logicalChannelType: OMIT,
            cn_DomainIdentity: OMIT
          }
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 3
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          sS_rlc_Info:
          {
            sS_ul_RLC_Mode:
            [
              dl_AM_RLC_Mode:
              {
                inSequenceDelivery: GcTRUE,
                receivingWindowSize: rw32,
                dl_RLC_StatusInfo:
                {
                  timerStatusProhibit: tsp200,
                  timerEPC: OMIT,
                  missingPDU_Indicator: GcTRUE,
                  timerStatusPeriodic: OMIT
                }
              }
            ],
            sS_dl_RLC_Mode:
            {
              dl_PayloadSize: 128,
              dl_RLCModeInfo:
              [
                ul_AM_RLC_Mode:
                {
                  transmissionRLC_Discard:
                  [
                    noDiscard: dat15
                  ],
                  transmissionWindowSize: tw32,
                  timerRST: tr500,
                  max_RST: rst1,
                  pollingInfo:
                  {
                    timerPollProhibit: tpp200,
                    timerPoll: tp200,
                    poll_PDU: OMIT,
                    poll_SDU: sdu1,
                    lastTransmissionPDU_Poll: GcTRUE,
                    lastRetransmissionPDU_Poll: GcTRUE,
                    pollWindow: pw99,
                    timerPollPeriodic: OMIT
                  }
                }
              ]
            }
          },
          rB_LogCH_Mapping:
          {
            uLlogicalChannelIdentity: 3,
            dLlogicalChannelIdentity: 3,
            logicalChannelType: OMIT,
            cn_DomainIdentity: OMIT
          }
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 4
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          sS_rlc_Info:
          {
            sS_ul_RLC_Mode:
            [
              dl_AM_RLC_Mode:
              {
                inSequenceDelivery: GcTRUE,
                receivingWindowSize: rw32,
                dl_RLC_StatusInfo:
                {
                  timerStatusProhibit: tsp200,
                  timerEPC: OMIT,
                  missingPDU_Indicator: GcTRUE,
                  timerStatusPeriodic: OMIT
                }
              }
            ],
            sS_dl_RLC_Mode:
            {
              dl_PayloadSize: 128,
              dl_RLCModeInfo:
              [
                ul_AM_RLC_Mode:
                {
                  transmissionRLC_Discard:
                  [
                    noDiscard: dat15
                  ],
                  transmissionWindowSize: tw32,
                  timerRST: tr500,
                  max_RST: rst1,
                  pollingInfo:
                  {
                    timerPollProhibit: tpp200,
                    timerPoll: tp200,
                    poll_PDU: OMIT,
                    poll_SDU: sdu1,
                    lastTransmissionPDU_Poll: GcTRUE,
                    lastRetransmissionPDU_Poll: GcTRUE,
                    pollWindow: pw99,
                    timerPollPeriodic: OMIT
                  }
                }
              ]
            }
          },
          rB_LogCH_Mapping:
          {
            uLlogicalChannelIdentity: 4,
            dLlogicalChannelIdentity: 4,
            logicalChannelType: OMIT,
            cn_DomainIdentity: OMIT
          }
        }
      ]
    }

TTCN PDU: AT_CmdCnf

(To search, click here and then press Ctrl+F)

    {
      result: OMIT,
      resultString: "<CR><LF>OK<CR><LF>",
      sMS_BlockMode: OMIT
    }

TTCN PDU: RLC_TR_DATA_IND

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: 0
      ],
      tM_message:
      [
        uL_CCCH_Message: PDU:
        {
          integrityCheckInfo: OMIT,
          message:
          [
            rrcConnectionRequest:
            {
              initialUE_Identity:
              [
                tmsi_and_LAI:
                {
                  tmsi: '00010001001000100011001101000100'B,
                  lai:
                  {
                    plmn_Identity:
                    {
                      mcc:
                      [
                        0,
                        0,
                        1
                      ],
                      mnc:
                      [
                        0,
                        1
                      ]
                    },
                    lac: '0000000000000001'B
                  }
                }
              ],
              establishmentCause: registration,
              protocolErrorIndicator: noError,
              measuredResultsOnRACH: OMIT,
              v3d0NonCriticalExtensions: OMIT
            }
          ]
        }
      ]
    }

TTCN PDU: RLC_UM_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: 0
      ],
      uM_message:
      [
        dL_CCCH_Message: PDU:
        {
          integrityCheckInfo: OMIT,
          message:
          [
            rrcConnectionSetup:
            [
              r3:
              {
                rrcConnectionSetup_r3:
                {
                  initialUE_Identity:
                  [
                    tmsi_and_LAI:
                    {
                      tmsi: '00010001001000100011001101000100'B,
                      lai:
                      {
                        plmn_Identity:
                        {
                          mcc:
                          [
                            0,
                            0,
                            1
                          ],
                          mnc:
                          [
                            0,
                            1
                          ]
                        },
                        lac: '0000000000000001'B
                      }
                    }
                  ],
                  rrc_TransactionIdentifier: 0,
                  activationTime: OMIT,
                  new_U_RNTI:
                  {
                    srnc_Identity: '000000000001'B,
                    s_RNTI: '00000000000000000001'B
                  },
                  new_c_RNTI: OMIT,
                  rrc_StateIndicator: cell_DCH,
                  utran_DRX_CycleLengthCoeff: 9,
                  capabilityUpdateRequirement:
                  {
                    ue_RadioCapabilityFDDUpdateRequirement: GcTRUE,
                    ue_RadioCapabilityTDDUpdateRequirement: GcFALSE,
                    systemSpecificCapUpdateReqList:
                    [
                      gsm
                    ]
                  },
                  srb_InformationSetupList:
                  [
                    {
                      rb_Identity: OMIT,
                      rlc_InfoChoice:
                      [
                        rlc_Info:
                        {
                          ul_RLC_Mode:
                          [
                            ul_UM_RLC_Mode:
                            {
                              transmissionRLC_Discard: OMIT
                            }
                          ],
                          dl_RLC_Mode:
                          [
                            dl_UM_RLC_Mode: NULL
                          ]
                        }
                      ],
                      rb_MappingInfo:
                      [
                        {
                          ul_LogicalChannelMappings:
                          [
                            oneLogicalChannel:
                            {
                              ul_TransportChannelType:
                              [
                                dch: 5
                              ],
                              logicalChannelIdentity: 1,
                              rlc_SizeList:
                              [
                                configured: NULL
                              ],
                              mac_LogicalChannelPriority: 1
                            }
                          ],
                          dl_LogicalChannelMappingList:
                          [
                            {
                              dl_TransportChannelType:
                              [
                                dch: 10
                              ],
                              logicalChannelIdentity: 1
                            }
                          ]
                        },

                        {
                          ul_LogicalChannelMappings:
                          [
                            oneLogicalChannel:
                            {
                              ul_TransportChannelType:
                              [
                                rach: NULL
                              ],
                              logicalChannelIdentity: 1,
                              rlc_SizeList:
                              [
                                explicitList:
                                [
                                  {
                                    rlc_SizeIndex: 1
                                  }
                                ]
                              ],
                              mac_LogicalChannelPriority: 1
                            }
                          ],
                          dl_LogicalChannelMappingList:
                          [
                            {
                              dl_TransportChannelType:
                              [
                                fach: NULL
                              ],
                              logicalChannelIdentity: 1
                            }
                          ]
                        }
                      ]
                    },

                    {
                      rb_Identity: OMIT,
                      rlc_InfoChoice:
                      [
                        rlc_Info:
                        {
                          ul_RLC_Mode:
                          [
                            ul_AM_RLC_Mode:
                            {
                              transmissionRLC_Discard:
                              [
                                noDiscard: dat15
                              ],
                              transmissionWindowSize: tw32,
                              timerRST: tr500,
                              max_RST: rst1,
                              pollingInfo:
                              {
                                timerPollProhibit: tpp200,
                                timerPoll: tp200,
                                poll_PDU: OMIT,
                                poll_SDU: sdu1,
                                lastTransmissionPDU_Poll: GcTRUE,
                                lastRetransmissionPDU_Poll: GcTRUE,
                                pollWindow: pw99,
                                timerPollPeriodic: OMIT
                              }
                            }
                          ],
                          dl_RLC_Mode:
                          [
                            dl_AM_RLC_Mode:
                            {
                              inSequenceDelivery: GcTRUE,
                              receivingWindowSize: rw32,
                              dl_RLC_StatusInfo:
                              {
                                timerStatusProhibit: tsp200,
                                timerEPC: OMIT,
                                missingPDU_Indicator: GcTRUE,
                                timerStatusPeriodic: OMIT
                              }
                            }
                          ]
                        }
                      ],
                      rb_MappingInfo:
                      [
                        {
                          ul_LogicalChannelMappings:
                          [
                            oneLogicalChannel:
                            {
                              ul_TransportChannelType:
                              [
                                dch: 5
                              ],
                              logicalChannelIdentity: 2,
                              rlc_SizeList:
                              [
                                configured: NULL
                              ],
                              mac_LogicalChannelPriority: 2
                            }
                          ],
                          dl_LogicalChannelMappingList:
                          [
                            {
                              dl_TransportChannelType:
                              [
                                dch: 10
                              ],
                              logicalChannelIdentity: 2
                            }
                          ]
                        },

                        {
                          ul_LogicalChannelMappings:
                          [
                            oneLogicalChannel:
                            {
                              ul_TransportChannelType:
                              [
                                rach: NULL
                              ],
                              logicalChannelIdentity: 2,
                              rlc_SizeList:
                              [
                                explicitList:
                                [
                                  {
                                    rlc_SizeIndex: 1
                                  }
                                ]
                              ],
                              mac_LogicalChannelPriority: 2
                            }
                          ],
                          dl_LogicalChannelMappingList:
                          [
                            {
                              dl_TransportChannelType:
                              [
                                fach: NULL
                              ],
                              logicalChannelIdentity: 2
                            }
                          ]
                        }
                      ]
                    },

                    {
                      rb_Identity: OMIT,
                      rlc_InfoChoice:
                      [
                        rlc_Info:
                        {
                          ul_RLC_Mode:
                          [
                            ul_AM_RLC_Mode:
                            {
                              transmissionRLC_Discard:
                              [
                                noDiscard: dat15
                              ],
                              transmissionWindowSize: tw32,
                              timerRST: tr500,
                              max_RST: rst1,
                              pollingInfo:
                              {
                                timerPollProhibit: tpp200,
                                timerPoll: tp200,
                                poll_PDU: OMIT,
                                poll_SDU: sdu1,
                                lastTransmissionPDU_Poll: GcTRUE,
                                lastRetransmissionPDU_Poll: GcTRUE,
                                pollWindow: pw99,
                                timerPollPeriodic: OMIT
                              }
                            }
                          ],
                          dl_RLC_Mode:
                          [
                            dl_AM_RLC_Mode:
                            {
                              inSequenceDelivery: GcTRUE,
                              receivingWindowSize: rw32,
                              dl_RLC_StatusInfo:
                              {
                                timerStatusProhibit: tsp200,
                                timerEPC: OMIT,
                                missingPDU_Indicator: GcTRUE,
                                timerStatusPeriodic: OMIT
                              }
                            }
                          ]
                        }
                      ],
                      rb_MappingInfo:
                      [
                        {
                          ul_LogicalChannelMappings:
                          [
                            oneLogicalChannel:
                            {
                              ul_TransportChannelType:
                              [
                                dch: 5
                              ],
                              logicalChannelIdentity: 3,
                              rlc_SizeList:
                              [
                                configured: NULL
                              ],
                              mac_LogicalChannelPriority: 3
                            }
                          ],
                          dl_LogicalChannelMappingList:
                          [
                            {
                              dl_TransportChannelType:
                              [
                                dch: 10
                              ],
                              logicalChannelIdentity: 3
                            }
                          ]
                        },

                        {
                          ul_LogicalChannelMappings:
                          [
                            oneLogicalChannel:
                            {
                              ul_TransportChannelType:
                              [
                                rach: NULL
                              ],
                              logicalChannelIdentity: 3,
                              rlc_SizeList:
                              [
                                explicitList:
                                [
                                  {
                                    rlc_SizeIndex: 1
                                  }
                                ]
                              ],
                              mac_LogicalChannelPriority: 3
                            }
                          ],
                          dl_LogicalChannelMappingList:
                          [
                            {
                              dl_TransportChannelType:
                              [
                                fach: NULL
                              ],
                              logicalChannelIdentity: 3
                            }
                          ]
                        }
                      ]
                    },

                    {
                      rb_Identity: OMIT,
                      rlc_InfoChoice:
                      [
                        rlc_Info:
                        {
                          ul_RLC_Mode:
                          [
                            ul_AM_RLC_Mode:
                            {
                              transmissionRLC_Discard:
                              [
                                noDiscard: dat15
                              ],
                              transmissionWindowSize: tw32,
                              timerRST: tr500,
                              max_RST: rst1,
                              pollingInfo:
                              {
                                timerPollProhibit: tpp200,
                                timerPoll: tp200,
                                poll_PDU: OMIT,
                                poll_SDU: sdu1,
                                lastTransmissionPDU_Poll: GcTRUE,
                                lastRetransmissionPDU_Poll: GcTRUE,
                                pollWindow: pw99,
                                timerPollPeriodic: OMIT
                              }
                            }
                          ],
                          dl_RLC_Mode:
                          [
                            dl_AM_RLC_Mode:
                            {
                              inSequenceDelivery: GcTRUE,
                              receivingWindowSize: rw32,
                              dl_RLC_StatusInfo:
                              {
                                timerStatusProhibit: tsp200,
                                timerEPC: OMIT,
                                missingPDU_Indicator: GcTRUE,
                                timerStatusPeriodic: OMIT
                              }
                            }
                          ]
                        }
                      ],
                      rb_MappingInfo:
                      [
                        {
                          ul_LogicalChannelMappings:
                          [
                            oneLogicalChannel:
                            {
                              ul_TransportChannelType:
                              [
                                dch: 5
                              ],
                              logicalChannelIdentity: 4,
                              rlc_SizeList:
                              [
                                configured: NULL
                              ],
                              mac_LogicalChannelPriority: 4
                            }
                          ],
                          dl_LogicalChannelMappingList:
                          [
                            {
                              dl_TransportChannelType:
                              [
                                dch: 10
                              ],
                              logicalChannelIdentity: 4
                            }
                          ]
                        },

                        {
                          ul_LogicalChannelMappings:
                          [
                            oneLogicalChannel:
                            {
                              ul_TransportChannelType:
                              [
                                rach: NULL
                              ],
                              logicalChannelIdentity: 4,
                              rlc_SizeList:
                              [
                                explicitList:
                                [
                                  {
                                    rlc_SizeIndex: 1
                                  }
                                ]
                              ],
                              mac_LogicalChannelPriority: 4
                            }
                          ],
                          dl_LogicalChannelMappingList:
                          [
                            {
                              dl_TransportChannelType:
                              [
                                fach: NULL
                              ],
                              logicalChannelIdentity: 4
                            }
                          ]
                        }
                      ]
                    }
                  ],
                  ul_CommonTransChInfo:
                  {
                    tfc_Subset: OMIT,
                    prach_TFCS: OMIT,
                    modeSpecificInfo:
                    [
                      fdd:
                      {
                        ul_TFCS:
                        [
                          normalTFCI_Signalling:
                          [
                            complete:
                            {
                              ctfcSize:
                              [
                                ctfc2Bit:
                                [
                                  {
                                    ctfc2: 0,
                                    powerOffsetInformation:
                                    {
                                      gainFactorInformation:
                                      [
                                        computedGainFactors: 0
                                      ],
                                      powerOffsetPp_m: OMIT
                                    }
                                  },

                                  {
                                    ctfc2: 1,
                                    powerOffsetInformation:
                                    {
                                      gainFactorInformation:
                                      [
                                        signalledGainFactors:
                                        {
                                          modeSpecificInfo:
                                          [
                                            fdd:
                                            {
                                              gainFactorBetaC: 11
                                            }
                                          ],
                                          gainFactorBetaD: 15,
                                          referenceTFC_ID: 0
                                        }
                                      ],
                                      powerOffsetPp_m: OMIT
                                    }
                                  }
                                ]
                              ]
                            }
                          ]
                        ]
                      }
                    ]
                  },
                  ul_AddReconfTransChInfoList:
                  [
                    {
                      ul_TransportChannelType: dch,
                      transportChannelIdentity: 5,
                      transportFormatSet:
                      [
                        dedicatedTransChTFS:
                        {
                          tti:
                          [
                            tti10:
                            [
                              {
                                rlc_Size:
                                [
                                  bitMode:
                                  [
                                    sizeType2:
                                    {
                                      part1: 2,
                                      part2: OMIT
                                    }
                                  ]
                                ],
                                numberOfTbSizeList:
                                [
                                  [
                                    zero: NULL
                                  ],

                                  [
                                    one: NULL
                                  ]
                                ],
                                logicalChannelList:
                                [
                                  allSizes: NULL
                                ]
                              }
                            ]
                          ],
                          semistaticTF_Information:
                          {
                            channelCodingType:
                            [
                              convolutional: third
                            ],
                            rateMatchingAttribute# 192 # crc_Size# crc16
                          }
                        }
                      ]
                    }
                  ]
                  # dl_CommonTransChInfo#
                  {
                    sccpch_TFCS# OMIT# modeSpecificInfo#
                    [
                      fdd#
                      {
                        dl_Parameters#
                        [
                          sameAsUL# NULL
                        ]
                      }
                    ]
                  }
                  # dl_AddReconfTransChInfoList#
                  [
                    {
                      dl_TransportChannelType# dch# dl_transportChannelIdentity# 10 # tfs_SignallingMode#
                      [
                        sameAsULTrCH#
                        {
                          ul_TransportChannelType# dch# ul_TransportChannelIdentity# 5
                        }
                      ]
                      # dch_QualityTarget#
                      {
                        bler_QualityValue# #20
                      }
                      # dummy# OMIT
                    }
                  ]
                  # frequencyInfo# OMIT# maxAllowedUL_TX_Power# OMIT# ul_ChannelRequirement#
                  [
                    ul_DPCH_Info#
                    {
                      ul_DPCH_PowerControlInfo#
                      [
                        fdd#
                        {
                          dpcch_PowerOffset# #40 # pc_Preamble# 1 # sRB_delay# 7 # powerControlAlgorithm#
                          [
                            algorithm1# 0
                          ]
                        }
                      ]
                      # modeSpecificInfo#
                      [
                        fdd#
                        {
                          scramblingCodeType# longSC# scramblingCode# 0 # numberOfDPDCH# OMIT# spreadingFactor# sf64# tfci_Existence# GcTRUE # numberOfFBI_Bits# OMIT# puncturingLimit# pl1
                        }
                      ]
                    }
                  ]
                  # dl_CommonInformation#
                  {
                    dl_DPCH_InfoCommon#
                    {
                      cfnHandling#
                      [
                        initialise#
                        {
                          cfntargetsfnframeoffset# OMIT
                        }
                      ]
                      # modeSpecificInfo#
                      [
                        fdd#
                        {
                          dl_DPCH_PowerControlInfo#
                          {
                            modeSpecificInfo#
                            [
                              fdd#
                              {
                                dpc_Mode# singleTPC
                              }
                            ]
                          }
                          # powerOffsetPilot_pdpdch# 0 # dl_rate_matching_restriction# OMIT# spreadingFactorAndPilot#
                          [
                            sfd128# pb4
                          ]
                          # positionFixedOrFlexible# fixed# tfci_Existence# GcFALSE
                        }
                      ]
                    }
                    # modeSpecificInfo#
                    [
                      fdd#
                      {
                        defaultDPCH_OffsetValue# 0 # dpch_CompressedModeInfo# OMIT# tx_DiversityMode# noDiversity# ssdt_Information# OMIT
                      }
                    ]
                  }
                  # dl_InformationPerRL_List#
                  [
                    {
                      modeSpecificInfo#
                      [
                        fdd#
                        {
                          primaryCPICH_Info#
                          {
                            primaryScramblingCode# 100
                          }
                          # pdsch_SHO_DCH_Info# OMIT# pdsch_CodeMapping# OMIT
                        }
                      ]
                      # dl_DPCH_InfoPerRL#
                      [
                        fdd#
                        {
                          pCPICH_UsageForChannelEst# mayBeUsed# dpch_FrameOffset# 0 # secondaryCPICH_Info# OMIT# dl_ChannelisationCodeList#
                          [
                            {
                              secondaryScramblingCode# 1 # sf_AndCodeNumber#
                              [
                                sf128# 0
                              ]
                              # scramblingCodeChange# noCodeChange
                            }
                          ]
                          # tpc_CombinationIndex# 0 # ssdt_CellIdentity# OMIT# closedLoopTimingAdjMode# OMIT
                        }
                      ]
                      # sccpch_InfoforFACH# OMIT
                    }
                  ]
                }
                # laterNonCriticalExtensions# OMIT
              }
            ]
          ]
        }
      ]
      # specialLI# GcTRUE
    }

TTCN PDU: RLC_AM_DATA_IND

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 2
      ],
      integrityResult:
      [
        integrityUsed: i_pass
      ],
      aM_message:
      [
        uL_DCCH_Message: PDU:
        {
          integrityCheckInfo: OMIT,
          message:
          [
            rrcConnectionSetupComplete:
            {
              rrc_TransactionIdentifier: 0,
              startList:
              [
                {
                  cn_DomainIdentity: ps_domain,
                  start_Value: '00000000000000000010'B
                },

                {
                  cn_DomainIdentity: cs_domain,
                  start_Value: '00000000000000000010'B
                }
              ],
              ue_RadioAccessCapability:
              {
                accessStratumReleaseIndicator: r99,
                pdcp_Capability:
                {
                  losslessSRNS_RelocationSupport: GcFALSE,
                  supportForRfc2507:
                  [
                    notSupported: NULL
                  ]
                },
                rlc_Capability:
                {
                  totalRLC_AM_BufferSize: kb50,
                  maximumRLC_WindowSize: mws2047,
                  maximumAM_EntityNumber: am6
                },
                transportChannelCapability:
                {
                  dl_TransChCapability:
                  {
                    maxNoBitsReceived: b8960,
                    maxConvCodeBitsReceived: b1280,
                    turboDecodingSupport:
                    [
                      supported: b8960
                    ],
                    maxSimultaneousTransChs: e8,
                    maxSimultaneousCCTrCH_Count: 1,
                    maxReceivedTransportBlocks: tb32,
                    maxNumberOfTFC: tfc128,
                    maxNumberOfTF: tf64
                  },
                  ul_TransChCapability:
                  {
                    maxNoBitsTransmitted: b3840,
                    maxConvCodeBitsTransmitted: b1280,
                    turboEncodingSupport:
                    [
                      supported: b3840
                    ],
                    maxSimultaneousTransChs: e8,
                    modeSpecificInfo:
                    [
                      fdd: NULL
                    ],
                    maxTransmittedBlocks: tb32,
                    maxNumberOfTFC: tfc64,
                    maxNumberOfTF: tf32
                  }
                },
                rf_Capability:
                {
                  fddRF_Capability:
                  {
                    ue_PowerClass: 4,
                    txRxFrequencySeparation: mhz190
                  },
                  tddRF_Capability: OMIT
                },
                physicalChannelCapability:
                {
                  fddPhysChCapability:
                  {
                    downlinkPhysChCapability:
                    {
                      maxNoDPCH_PDSCH_Codes: 1,
                      maxNoPhysChBitsReceived: b9600,
                      supportForSF_512: GcFALSE,
                      supportOfPDSCH: GcFALSE,
                      simultaneousSCCPCH_DPCH_Reception:
                      [
                        notSupported: NULL
                      ]
                    },
                    uplinkPhysChCapability:
                    {
                      maxNoDPDCH_BitsTransmitted: b4800,
                      supportOfPCPCH: GcFALSE
                    }
                  },
                  tddPhysChCapability: OMIT
                },
                ue_MultiModeRAT_Capability:
                {
                  multiRAT_CapabilityList:
                  {
                    supportOfGSM: GcFALSE,
                    supportOfMulticarrier: GcFALSE
                  },
                  multiModeCapability: fdd
                },
                securityCapability:
                {
                  cipheringAlgorithmCap: '0000000000000011'B,
                  integrityProtectionAlgorithmCap: '0000000000000010'B
                },
                ue_positioning_Capability:
                {
                  standaloneLocMethodsSupported: GcFALSE,
                  ue_BasedOTDOA_Supported: GcFALSE,
                  networkAssistedGPS_Supported: noNetworkAssistedGPS,
                  supportForUE_GPS_TimingOfCellFrames: GcFALSE,
                  supportForIPDL: GcFALSE
                },
                measurementCapability:
                {
                  downlinkCompressedMode:
                  {
                    fdd_Measurements: GcTRUE,
                    tdd_Measurements: OMIT,
                    gsm_Measurements:
                    {
                      gsm900: GcTRUE,
                      dcs1800: GcTRUE,
                      gsm1900: GcTRUE
                    },
                    multiCarrierMeasurements: GcFALSE
                  },
                  uplinkCompressedMode:
                  {
                    fdd_Measurements: GcTRUE,
                    tdd_Measurements: OMIT,
                    gsm_Measurements:
                    {
                      gsm900: GcTRUE,
                      dcs1800: GcTRUE,
                      gsm1900: GcTRUE
                    },
                    multiCarrierMeasurements: GcFALSE
                  }
                }
              },
              ue_RATSpecificCapability: OMIT,
              v370NonCriticalExtensions: OMIT
            }
          ]
        }
      ]
    }

TTCN PDU: RRC_DataInd

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      rB_Id: 3,
      ch: OMIT,
      sapId: OMIT,
      cN_Domain: 1,
      start: '00000000000000000010'B,
      msg: PDU:
      {
        skipIndicator: '0000'B,
        gMMProtocolDiscriminator: '1000'B,
        msgType: '00000001'B,
        msNetworkCap:
        {
          iel: '02'O,
          value: 'E540'O
        },
        gprsCiphKeySeqNo:
        {
          spare1: '0'B,
          keySeq: '000'B
        },
        attachType:
        {
          for: '0'B,
          type: '001'B
        },
        drxParameter:
        {
          splitPGcycleCode: '00000111'B,
          cnDRXcoef: '0000'B,
          splitOnCCCH: '0'B,
          nonDRXtimer: '100'B
        },
        ptmsiORimsi:
        {
          iel: '05'O,
          iDigit1: '1111'B,
          oddEvenInd: '0'B,
          typeOfId: '100'B,
          otherDigits: '12345678'O
        },
        oldRAI:
        {
          plmn: '00F110'O,
          lac: '0001'O,
          rac: '05'O
        },
        msRadioAccessCap:
        {
          iel: '0B'O,
          value: '15F38233542A332644A198'O
        },
        oldPTMSI_Signature: OMIT,
        readyTimer:
        {
          iei: '00010111'B,
          unit: '000'B,
          value: '10110'B
        },
        tmsiStatus: OMIT
      }
    }

TTCN PDU: RRC_DataReq

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      rB_Id: 3,
      ch: OMIT,
      sapId: OMIT,
      cN_Domain: 1,
      msg: PDU:
      {
        skipIndicator: '0000'B,
        gMMProtocolDiscriminator: '1000'B,
        msgType: '00010010'B,
        imeisvReq:
        {
          spare1: '0'B,
          value: '000'B
        },
        ciphAlgorithm:
        {
          spare1: '0'B,
          algorithm: '001'B
        },
        acRefNo:
        {
          value: '0011'B
        },
        forceToStandby:
        {
          spare: '0'B,
          value: '000'B
        },
        authRand:
        {
          iei: '00100001'B,
          randValue: '01010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101'B
        },
        gprsCiphKeySeqNo:
        {
          iei: '1000'B,
          spare1: '0'B,
          keySeq: '001'B
        },
        aUTN:
        {
          iei: '00101000'B,
          iel: '10'O,
          aUTN: '01100110000100010000000000110011001000101101110100000000000000000101010101000100011101110110011000010001000000000011001100100010'B
        }
      }
    }

TTCN PDU: Assignment:[3] tcv_TmpAuthAndCiphRs

(To search, click here and then press Ctrl+F)

    := PDU:
    {
      skipIndicator: '0000'B,
      gMMProtocolDiscriminator: '1000'B,
      msgType: '00010011'B,
      spare4: '0000'B,
      acRefNo:
      {
        value: '0011'B
      },
      authRsp:
      {
        iei: '00100010'B,
        value: '01010101010001000111011101100110'B
      },
      imeisv: OMIT,
      authRspExt:
      {
        iei: '00101001'B,
        iel: '04'O,
        rES: '00010001000000000011001100100010'B
      }
    }

TTCN PDU: RRC_DataInd

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      rB_Id: 3,
      ch: OMIT,
      sapId: OMIT,
      cN_Domain: 1,
      start: OMIT,
      msg: PDU:
      {
        skipIndicator: '0000'B,
        gMMProtocolDiscriminator: '1000'B,
        msgType: '00010011'B,
        spare4: '0000'B,
        acRefNo:
        {
          value: '0011'B
        },
        authRsp:
        {
          iei: '00100010'B,
          value: '01010101010001000111011101100110'B
        },
        imeisv: OMIT,
        authRspExt:
        {
          iei: '00101001'B,
          iel: '04'O,
          rES: '00010001000000000011001100100010'B
        }
      }
    }

TTCN PDU: CRLC_SecurityMode_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      rlcSecurityInfo:
      {
        cn_DomainIdentity: ps_domain,
        startValue: '00000000000000000000'B,
        cipheringKey: OMIT,
        integrityKey: '01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100'B,
        gsmCipheringKey: OMIT
      }
    }

TTCN PDU: CRLC_SetRRC_MessageSN_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: 0
      ],
      count_I_LSB_UL: OMIT,
      count_I_LSB_DL: 0
    }

TTCN PDU: CRLC_SetRRC_MessageSN_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 1
      ],
      count_I_LSB_UL: OMIT,
      count_I_LSB_DL: 0
    }

TTCN PDU: CRLC_SetRRC_MessageSN_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 2
      ],
      count_I_LSB_UL: OMIT,
      count_I_LSB_DL: 0
    }

TTCN PDU: CRLC_SetRRC_MessageSN_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 3
      ],
      count_I_LSB_UL: OMIT,
      count_I_LSB_DL: 0
    }

TTCN PDU: CRLC_SetRRC_MessageSN_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 4
      ],
      count_I_LSB_UL: OMIT,
      count_I_LSB_DL: 0
    }

TTCN PDU: CRLC_Integrity_Activate_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      cn_DomainIdentity: ps_domain,
      integrityActivationInfo:
      [
        integrityProtectionModeInfo:
        {
          integrityProtectionModeCommand:
          [
            startIntegrityProtection:
            {
              integrityProtInitNumber: '00001111000011110000111100001111'B
            }
          ],
          integrityProtectionAlgorithm: uia1
        }
      ]
    }

TTCN PDU: CRLC_Integrity_Activate_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      cn_DomainIdentity: ps_domain,
      integrityActivationInfo:
      [
        ul_IntegProtActivationInfo:
        [
          {
            rb_Identity: 2,
            rrc_MessageSequenceNumber: 0
          }
        ]
      ]
    }

TTCN PDU: RLC_AM_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 2
      ],
      confirmationRequest:
      [
        noConfirmationRequest: NULL
      ],
      aM_message:
      [
        dL_DCCH_Message: PDU:
        {
          integrityCheckInfo:
          {
            messageAuthenticationCode: '00011101101101011011110100000101'B,
            rrc_MessageSequenceNumber: 1
          },
          message:
          [
            securityModeCommand:
            [
              r3:
              {
                securityModeCommand_r3:
                {
                  rrc_TransactionIdentifier: 0,
                  securityCapability:
                  {
                    cipheringAlgorithmCap: '0000000000000011'B,
                    integrityProtectionAlgorithmCap: '0000000000000010'B
                  },
                  cipheringModeInfo: OMIT,
                  integrityProtectionModeInfo:
                  {
                    integrityProtectionModeCommand:
                    [
                      startIntegrityProtection:
                      {
                        integrityProtInitNumber: '00001111000011110000111100001111'B
                      }
                    ],
                    integrityProtectionAlgorithm: uia1
                  },
                  cn_DomainIdentity: ps_domain,
                  ue_SystemSpecificSecurityCap: OMIT
                },
                laterNonCriticalExtensions: OMIT
              }
            ]
          ]
        }
      ]
    }

TTCN PDU: RLC_AM_DATA_IND

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 2
      ],
      integrityResult:
      [
        integrityUsed: i_pass
      ],
      aM_message:
      [
        uL_DCCH_Message: PDU:
        {
          integrityCheckInfo:
          {
            messageAuthenticationCode: '10001011001000110111110011100010'B,
            rrc_MessageSequenceNumber: 1
          },
          message:
          [
            securityModeComplete:
            {
              rrc_TransactionIdentifier: 0,
              ul_IntegProtActivationInfo:
              {
                rrc_MessageSequenceNumberList:
                [
                  0,
                  0,
                  0,
                  0,
                  0
                ]
              },
              rb_UL_CiphActivationTimeInfo: OMIT,
              laterNonCriticalExtensions: OMIT
            }
          ]
        }
      ]
    }

TTCN PDU: CRLC_Integrity_Activate_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      cn_DomainIdentity: ps_domain,
      integrityActivationInfo:
      [
        ul_IntegProtActivationInfo:
        [
          {
            rb_Identity: 0,
            rrc_MessageSequenceNumber: 0
          },

          {
            rb_Identity: 1,
            rrc_MessageSequenceNumber: 0
          },

          {
            rb_Identity: 3,
            rrc_MessageSequenceNumber: 0
          },

          {
            rb_Identity: 4,
            rrc_MessageSequenceNumber: 0
          }
        ]
      ]
    }

TTCN PDU: RRC_DataReq

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      rB_Id: 3,
      ch: OMIT,
      sapId: OMIT,
      cN_Domain: 1,
      msg: PDU:
      {
        skipIndicator: '0000'B,
        gMMProtocolDiscriminator: '1000'B,
        msgType: '00000010'B,
        forceToStandby:
        {
          spare: '0'B,
          value: '000'B
        },
        attachResult:
        {
          spare: '0'B,
          result: '001'B
        },
        periodicRAupdateTimer:
        {
          unit: '111'B,
          value: '00000'B
        },
        spare: '0000'B,
        radioPrioSMS:
        {
          spare: '0'B,
          value: '100'B
        },
        rai:
        {
          plmn: '00F110'O,
          lac: '0001'O,
          rac: '05'O
        },
        ptmsiSignature: OMIT,
        negReadyTimer: OMIT,
        allocatedPTMSI: OMIT,
        msIdentity: OMIT,
        gmmCause: OMIT,
        t3302Value: OMIT,
        cellNotification: OMIT,
        equivalentPLMN: OMIT
      }
    }

TTCN PDU: RLC_UM_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 1
      ],
      uM_message:
      [
        dL_DCCH_Message: PDU:
        {
          integrityCheckInfo:
          {
            messageAuthenticationCode: '11101100100111000001011111010011'B,
            rrc_MessageSequenceNumber: 1
          },
          message:
          [
            rrcConnectionRelease:
            [
              r3:
              {
                rrcConnectionRelease_r3:
                {
                  rrc_TransactionIdentifier: 0,
                  n_308: 1,
                  releaseCause: normalEvent,
                  rplmn_information: OMIT
                },
                laterNonCriticalExtensions: OMIT
              }
            ]
          ]
        }
      ],
      specialLI: GcFALSE
    }

TTCN PDU: RLC_UM_DATA_IND

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 1
      ],
      integrityResult:
      [
        integrityUsed: i_pass
      ],
      uM_message:
      [
        uL_DCCH_Message: PDU:
        {
          integrityCheckInfo:
          {
            messageAuthenticationCode: '11110111111000101100001011001110'B,
            rrc_MessageSequenceNumber: 1
          },
          message:
          [
            rrcConnectionReleaseComplete:
            {
              rrc_TransactionIdentifier: 0,
              errorIndication: OMIT,
              laterNonCriticalExtensions: OMIT
            }
          ]
        }
      ]
    }

TTCN PDU: RLC_UM_DATA_IND

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 1
      ],
      integrityResult:
      [
        integrityUsed: i_pass
      ],
      uM_message:
      [
        uL_DCCH_Message: PDU:
        {
          integrityCheckInfo:
          {
            messageAuthenticationCode: '10111001101000110000011111000000'B,
            rrc_MessageSequenceNumber: 2
          },
          message:
          [
            rrcConnectionReleaseComplete:
            {
              rrc_TransactionIdentifier: 0,
              errorIndication: OMIT,
              laterNonCriticalExtensions: OMIT
            }
          ]
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 1
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 2
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 3
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 4
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 1
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          sS_rlc_Info:
          {
            sS_ul_RLC_Mode:
            [
              dl_UM_RLC_Mode: NULL
            ],
            sS_dl_RLC_Mode:
            {
              dl_PayloadSize: 136,
              dl_RLCModeInfo:
              [
                ul_UM_RLC_Mode:
                {
                  transmissionRLC_Discard:
                  [
                    timerBasedNoExplicit: dt100
                  ]
                }
              ]
            }
          },
          rB_LogCH_Mapping:
          {
            uLlogicalChannelIdentity: 1,
            dLlogicalChannelIdentity: 1,
            logicalChannelType: OMIT,
            cn_DomainIdentity: OMIT
          }
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 2
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          sS_rlc_Info:
          {
            sS_ul_RLC_Mode:
            [
              dl_AM_RLC_Mode:
              {
                inSequenceDelivery: GcTRUE,
                receivingWindowSize: rw32,
                dl_RLC_StatusInfo:
                {
                  timerStatusProhibit: tsp200,
                  timerEPC: OMIT,
                  missingPDU_Indicator: GcTRUE,
                  timerStatusPeriodic: OMIT
                }
              }
            ],
            sS_dl_RLC_Mode:
            {
              dl_PayloadSize: 128,
              dl_RLCModeInfo:
              [
                ul_AM_RLC_Mode:
                {
                  transmissionRLC_Discard:
                  [
                    noDiscard: dat15
                  ],
                  transmissionWindowSize: tw32,
                  timerRST: tr500,
                  max_RST: rst1,
                  pollingInfo:
                  {
                    timerPollProhibit: tpp200,
                    timerPoll: tp200,
                    poll_PDU: OMIT,
                    poll_SDU: sdu1,
                    lastTransmissionPDU_Poll: GcTRUE,
                    lastRetransmissionPDU_Poll: GcTRUE,
                    pollWindow: pw99,
                    timerPollPeriodic: OMIT
                  }
                }
              ]
            }
          },
          rB_LogCH_Mapping:
          {
            uLlogicalChannelIdentity: 2,
            dLlogicalChannelIdentity: 2,
            logicalChannelType: OMIT,
            cn_DomainIdentity: OMIT
          }
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 3
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          sS_rlc_Info:
          {
            sS_ul_RLC_Mode:
            [
              dl_AM_RLC_Mode:
              {
                inSequenceDelivery: GcTRUE,
                receivingWindowSize: rw32,
                dl_RLC_StatusInfo:
                {
                  timerStatusProhibit: tsp200,
                  timerEPC: OMIT,
                  missingPDU_Indicator: GcTRUE,
                  timerStatusPeriodic: OMIT
                }
              }
            ],
            sS_dl_RLC_Mode:
            {
              dl_PayloadSize: 128,
              dl_RLCModeInfo:
              [
                ul_AM_RLC_Mode:
                {
                  transmissionRLC_Discard:
                  [
                    noDiscard: dat15
                  ],
                  transmissionWindowSize: tw32,
                  timerRST: tr500,
                  max_RST: rst1,
                  pollingInfo:
                  {
                    timerPollProhibit: tpp200,
                    timerPoll: tp200,
                    poll_PDU: OMIT,
                    poll_SDU: sdu1,
                    lastTransmissionPDU_Poll: GcTRUE,
                    lastRetransmissionPDU_Poll: GcTRUE,
                    pollWindow: pw99,
                    timerPollPeriodic: OMIT
                  }
                }
              ]
            }
          },
          rB_LogCH_Mapping:
          {
            uLlogicalChannelIdentity: 3,
            dLlogicalChannelIdentity: 3,
            logicalChannelType: OMIT,
            cn_DomainIdentity: OMIT
          }
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 4
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          sS_rlc_Info:
          {
            sS_ul_RLC_Mode:
            [
              dl_AM_RLC_Mode:
              {
                inSequenceDelivery: GcTRUE,
                receivingWindowSize: rw32,
                dl_RLC_StatusInfo:
                {
                  timerStatusProhibit: tsp200,
                  timerEPC: OMIT,
                  missingPDU_Indicator: GcTRUE,
                  timerStatusPeriodic: OMIT
                }
              }
            ],
            sS_dl_RLC_Mode:
            {
              dl_PayloadSize: 128,
              dl_RLCModeInfo:
              [
                ul_AM_RLC_Mode:
                {
                  transmissionRLC_Discard:
                  [
                    noDiscard: dat15
                  ],
                  transmissionWindowSize: tw32,
                  timerRST: tr500,
                  max_RST: rst1,
                  pollingInfo:
                  {
                    timerPollProhibit: tpp200,
                    timerPoll: tp200,
                    poll_PDU: OMIT,
                    poll_SDU: sdu1,
                    lastTransmissionPDU_Poll: GcTRUE,
                    lastRetransmissionPDU_Poll: GcTRUE,
                    pollWindow: pw99,
                    timerPollPeriodic: OMIT
                  }
                }
              ]
            }
          },
          rB_LogCH_Mapping:
          {
            uLlogicalChannelIdentity: 4,
            dLlogicalChannelIdentity: 4,
            logicalChannelType: OMIT,
            cn_DomainIdentity: OMIT
          }
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 1
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 2
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 3
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 4
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CMAC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        physicalChannelIdentity: 26
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CMAC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        physicalChannelIdentity: 20
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CPHY_TrCH_Release_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 26
      ],
      trchConfigType:
      [
        dch: normal
      ]
    }

TTCN PDU: CPHY_TrCH_Release_CNF

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 26
      ]
    }

TTCN PDU: CPHY_TrCH_Release_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 20
      ],
      trchConfigType:
      [
        dch: normal
      ]
    }

TTCN PDU: CPHY_TrCH_Release_CNF

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 20
      ]
    }

TTCN PDU: CPHY_RL_Setup_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        physicalChannelIdentity: 26
      ],
      ratType: fdd,
      setupMessage:
      {
        physicalChannelInfo:
        [
          dPCHInfo:
          {
            ul_DPCHInfo: OMIT,
            dl_DPCHInfo:
            {
              dl_CommonInformation:
              {
                dl_DPCH_InfoCommon:
                {
                  cfnHandling:
                  [
                    initialise:
                    {
                      cfntargetsfnframeoffset: OMIT
                    }
                  ],
                  modeSpecificInfo:
                  [
                    fdd:
                    {
                      dl_DPCH_PowerControlInfo:
                      {
                        modeSpecificInfo:
                        [
                          fdd:
                          {
                            dpc_Mode: singleTPC
                          }
                        ]
                      },
                      powerOffsetPilot_pdpdch: 0,
                      dl_rate_matching_restriction: OMIT,
                      spreadingFactorAndPilot:
                      [
                        sfd128: pb4
                      ],
                      positionFixedOrFlexible: fixed,
                      tfci_Existence: GcFALSE
                    }
                  ]
                },
                modeSpecificInfo:
                [
                  fdd:
                  {
                    defaultDPCH_OffsetValue: 0,
                    dpch_CompressedModeInfo: OMIT,
                    tx_DiversityMode: noDiversity,
                    ssdt_Information: OMIT
                  }
                ]
              },
              dl_DPCH_InfoPerRL:
              [
                fdd:
                {
                  pCPICH_UsageForChannelEst: mayBeUsed,
                  dpch_FrameOffset: 0,
                  secondaryCPICH_Info: OMIT,
                  dl_ChannelisationCodeList:
                  [
                    {
                      secondaryScramblingCode: 1,
                      sf_AndCodeNumber:
                      [
                        sf128: 0
                      ],
                      scramblingCodeChange: OMIT
                    }
                  ],
                  tpc_CombinationIndex: 0,
                  ssdt_CellIdentity: OMIT,
                  closedLoopTimingAdjMode: OMIT
                }
              ],
              powerOffsetOfTFCI_PO1: 0,
              powerOffsetOfTPC_PO2: 0,
              powerOffsetOfPILOT_PO3: 0,
              dl_TxPower: -5,
              dl_TxPowerMax: 15,
              dl_TxPowerMin: -35
            }
          }
        ]
      }
    }

TTCN PDU: CPHY_TrCH_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        physicalChannelIdentity: 26
      ],
      ratType: fdd,
      trchConfigType:
      [
        dch: normal
      ],
      configMessage:
      {
        activationTime:
        [
          activateNow: NULL
        ],
        ulconnectedTrCHList: OMIT,
        ulTFCS: OMIT,
        dlconnectedTrCHList:
        [
          {
            trchid: 10,
            dl_TransportChannelType: dch,
            transportChannelInfo:
            {
              tti:
              [
                tti10:
                [
                  {
                    tb_Size: 148,
                    numberOfTbSizeList:
                    [
                      [
                        zero: NULL
                      ],

                      [
                        one: NULL
                      ]
                    ],
                    logicalChannelList:
                    [
                      allSizes: NULL
                    ]
                  }
                ]
              ],
              semistaticTF_Information:
              {
                channelCodingType:
                [
                  convolutional: third
                ],
                rateMatchingAttribute# 192 # crc_Size# crc16
              }
            }
          }
        ]
        # dlTFCS#
        [
          normalTFCI_Signalling#
          [
            complete#
            {
              ctfcSize#
              [
                ctfc2Bit#
                [
                  {
                    ctfc2# 0 # powerOffsetInformation#
                    {
                      gainFactorInformation#
                      [
                        computedGainFactors# 0
                      ]
                      # powerOffsetPp_m# OMIT
                    }
                  }
                  #
                  {
                    ctfc2# 1 # powerOffsetInformation#
                    {
                      gainFactorInformation#
                      [
                        signalledGainFactors#
                        {
                          modeSpecificInfo#
                          [
                            fdd#
                            {
                              gainFactorBetaC# 11
                            }
                          ]
                          # gainFactorBetaD# 15 # referenceTFC_ID# 0
                        }
                      ]
                      # powerOffsetPp_m# OMIT
                    }
                  }
                ]
              ]
            }
          ]
        ]
      }
    }

TTCN PDU: CPHY_TrCH_Config_CNF

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        physicalChannelIdentity: 26
      ]
    }

TTCN PDU: CMAC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        physicalChannelIdentity: 26
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          activationTime:
          [
            activateNow: NULL
          ],
          uE_Info:
          {
            u_RNTI: OMIT,
            c_RNTI: OMIT
          },
          trCHInfo:
          {
            ulconnectedTrCHList: OMIT,
            ulTFCS: OMIT,
            dlconnectedTrCHList:
            [
              {
                trchid: 10,
                transportChannelInfo:
                {
                  tti:
                  [
                    tti10:
                    [
                      {
                        tb_Size: 148,
                        numberOfTbSizeList:
                        [
                          [
                            zero: NULL
                          ],

                          [
                            one: NULL
                          ]
                        ],
                        logicalChannelList:
                        [
                          allSizes: NULL
                        ]
                      }
                    ]
                  ],
                  semistaticTF_Information:
                  {
                    channelCodingType:
                    [
                      convolutional: third
                    ],
                    rateMatchingAttribute# 192 # crc_Size# crc16
                  }
                }
              }
            ]
            # dlTFCS#
            [
              normalTFCI_Signalling#
              [
                complete#
                {
                  ctfcSize#
                  [
                    ctfc2Bit#
                    [
                      {
                        ctfc2# 0 # powerOffsetInformation#
                        {
                          gainFactorInformation#
                          [
                            computedGainFactors# 0
                          ]
                          # powerOffsetPp_m# OMIT
                        }
                      }
                      #
                      {
                        ctfc2# 1 # powerOffsetInformation#
                        {
                          gainFactorInformation#
                          [
                            signalledGainFactors#
                            {
                              modeSpecificInfo#
                              [
                                fdd#
                                {
                                  gainFactorBetaC# 11
                                }
                              ]
                              # gainFactorBetaD# 15 # referenceTFC_ID# 0
                            }
                          ]
                          # powerOffsetPp_m# OMIT
                        }
                      }
                    ]
                  ]
                }
              ]
            ]
          }
          # trCH_LogCHMapping#
          {
            ulconnectedTrCHList# OMIT# dlconnectedTrCHList#
            [
              {
                trchid# 10 # trCH_LogCHMappingList#
                [
                  {
                    logicalChannel_Mapping#
                    [
                      dl_LogicalChannelMapping#
                      {
                        macHeaderManipulation# normalMacHeader# dl_TransportChannelType# dch# logicalChannelIdentity# 1 # logicalChannelType# dCCH# rlc_SizeList#
                        [
                          configured# NULL
                        ]
                        # mac_LogicalChannelPriority# 1
                      }
                    ]
                    # rB_Identity# 1 # cn_DomainIdentity# OMIT
                  }
                  #
                  {
                    logicalChannel_Mapping#
                    [
                      dl_LogicalChannelMapping#
                      {
                        macHeaderManipulation# normalMacHeader# dl_TransportChannelType# dch# logicalChannelIdentity# 2 # logicalChannelType# dCCH# rlc_SizeList#
                        [
                          configured# NULL
                        ]
                        # mac_LogicalChannelPriority# 2
                      }
                    ]
                    # rB_Identity# 2 # cn_DomainIdentity# OMIT
                  }
                  #
                  {
                    logicalChannel_Mapping#
                    [
                      dl_LogicalChannelMapping#
                      {
                        macHeaderManipulation# normalMacHeader# dl_TransportChannelType# dch# logicalChannelIdentity# 3 # logicalChannelType# dCCH# rlc_SizeList#
                        [
                          configured# NULL
                        ]
                        # mac_LogicalChannelPriority# 3
                      }
                    ]
                    # rB_Identity# 3 # cn_DomainIdentity# OMIT
                  }
                  #
                  {
                    logicalChannel_Mapping#
                    [
                      dl_LogicalChannelMapping#
                      {
                        macHeaderManipulation# normalMacHeader# dl_TransportChannelType# dch# logicalChannelIdentity# 4 # logicalChannelType# dCCH# rlc_SizeList#
                        [
                          configured# NULL
                        ]
                        # mac_LogicalChannelPriority# 4
                      }
                    ]
                    # rB_Identity# 4 # cn_DomainIdentity# OMIT
                  }
                ]
              }
            ]
          }
        }
      ]
    }

TTCN PDU: CPHY_RL_Setup_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        physicalChannelIdentity: 20
      ],
      ratType: fdd,
      setupMessage:
      {
        physicalChannelInfo:
        [
          dPCHInfo:
          {
            ul_DPCHInfo:
            {
              ul_DPCH_PowerControlInfo:
              [
                fdd:
                {
                  dpcch_PowerOffset: -40,
                  pc_Preamble: 1,
                  sRB_delay: 7,
                  powerControlAlgorithm:
                  [
                    algorithm1: 0
                  ]
                }
              ],
              modeSpecificInfo:
              [
                fdd:
                {
                  scramblingCodeType: longSC,
                  scramblingCode: 1000,
                  numberOfDPDCH: OMIT,
                  spreadingFactor: sf64,
                  tfci_Existence: GcTRUE,
                  numberOfFBI_Bits: OMIT,
                  puncturingLimit: pl1
                }
              ]
            },
            dl_DPCHInfo: OMIT
          }
        ]
      }
    }

TTCN PDU: CPHY_TrCH_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        physicalChannelIdentity: 20
      ],
      ratType: fdd,
      trchConfigType:
      [
        dch: normal
      ],
      configMessage:
      {
        activationTime:
        [
          activateNow: NULL
        ],
        ulconnectedTrCHList:
        [
          {
            trchid: 5,
            ul_TransportChannelType: dch,
            transportChannelInfo:
            {
              tti:
              [
                tti10:
                [
                  {
                    tb_Size: 148,
                    numberOfTbSizeList:
                    [
                      [
                        zero: NULL
                      ],

                      [
                        one: NULL
                      ]
                    ],
                    logicalChannelList:
                    [
                      allSizes: NULL
                    ]
                  }
                ]
              ],
              semistaticTF_Information:
              {
                channelCodingType:
                [
                  convolutional: third
                ],
                rateMatchingAttribute# 192 # crc_Size# crc16
              }
            }
          }
        ]
        # ulTFCS#
        [
          normalTFCI_Signalling#
          [
            complete#
            {
              ctfcSize#
              [
                ctfc2Bit#
                [
                  {
                    ctfc2# 0 # powerOffsetInformation# OMIT
                  }
                  #
                  {
                    ctfc2# 1 # powerOffsetInformation# OMIT
                  }
                ]
              ]
            }
          ]
        ]
        # dlconnectedTrCHList# OMIT# dlTFCS# OMIT
      }
    }

TTCN PDU: CPHY_TrCH_Config_CNF

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        physicalChannelIdentity: 20
      ]
    }

TTCN PDU: CMAC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        physicalChannelIdentity: 20
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          activationTime:
          [
            activateNow: NULL
          ],
          uE_Info:
          {
            u_RNTI: OMIT,
            c_RNTI: OMIT
          },
          trCHInfo:
          {
            ulconnectedTrCHList:
            [
              {
                trchid: 5,
                transportChannelInfo:
                {
                  tti:
                  [
                    tti10:
                    [
                      {
                        tb_Size: 148,
                        numberOfTbSizeList:
                        [
                          [
                            zero: NULL
                          ],

                          [
                            one: NULL
                          ]
                        ],
                        logicalChannelList:
                        [
                          allSizes: NULL
                        ]
                      }
                    ]
                  ],
                  semistaticTF_Information:
                  {
                    channelCodingType:
                    [
                      convolutional: third
                    ],
                    rateMatchingAttribute# 192 # crc_Size# crc16
                  }
                }
              }
            ]
            # ulTFCS#
            [
              normalTFCI_Signalling#
              [
                complete#
                {
                  ctfcSize#
                  [
                    ctfc2Bit#
                    [
                      {
                        ctfc2# 0 # powerOffsetInformation# OMIT
                      }
                      #
                      {
                        ctfc2# 1 # powerOffsetInformation# OMIT
                      }
                    ]
                  ]
                }
              ]
            ]
            # dlconnectedTrCHList# OMIT# dlTFCS# OMIT
          }
          # trCH_LogCHMapping#
          {
            ulconnectedTrCHList#
            [
              {
                trchid# 5 # trCH_LogCHMappingList#
                [
                  {
                    logicalChannel_Mapping#
                    [
                      ul_LogicalChannelMapping#
                      {
                        macHeaderManipulation# normalMacHeader# ul_TransportChannelType# dch# logicalChannelIdentity# 1 # logicalChannelType# dCCH
                      }
                    ]
                    # rB_Identity# 1 # cn_DomainIdentity# OMIT
                  }
                  #
                  {
                    logicalChannel_Mapping#
                    [
                      ul_LogicalChannelMapping#
                      {
                        macHeaderManipulation# normalMacHeader# ul_TransportChannelType# dch# logicalChannelIdentity# 2 # logicalChannelType# dCCH
                      }
                    ]
                    # rB_Identity# 2 # cn_DomainIdentity# OMIT
                  }
                  #
                  {
                    logicalChannel_Mapping#
                    [
                      ul_LogicalChannelMapping#
                      {
                        macHeaderManipulation# normalMacHeader# ul_TransportChannelType# dch# logicalChannelIdentity# 3 # logicalChannelType# dCCH
                      }
                    ]
                    # rB_Identity# 3 # cn_DomainIdentity# OMIT
                  }
                  #
                  {
                    logicalChannel_Mapping#
                    [
                      ul_LogicalChannelMapping#
                      {
                        macHeaderManipulation# normalMacHeader# ul_TransportChannelType# dch# logicalChannelIdentity# 4 # logicalChannelType# dCCH
                      }
                    ]
                    # rB_Identity# 4 # cn_DomainIdentity# OMIT
                  }
                ]
              }
            ]
            # dlconnectedTrCHList# OMIT
          }
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 1
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          sS_rlc_Info:
          {
            sS_ul_RLC_Mode:
            [
              dl_UM_RLC_Mode: NULL
            ],
            sS_dl_RLC_Mode:
            {
              dl_PayloadSize: 136,
              dl_RLCModeInfo:
              [
                ul_UM_RLC_Mode:
                {
                  transmissionRLC_Discard:
                  [
                    timerBasedNoExplicit: dt100
                  ]
                }
              ]
            }
          },
          rB_LogCH_Mapping:
          {
            uLlogicalChannelIdentity: 1,
            dLlogicalChannelIdentity: 1,
            logicalChannelType: OMIT,
            cn_DomainIdentity: OMIT
          }
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 2
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          sS_rlc_Info:
          {
            sS_ul_RLC_Mode:
            [
              dl_AM_RLC_Mode:
              {
                inSequenceDelivery: GcTRUE,
                receivingWindowSize: rw32,
                dl_RLC_StatusInfo:
                {
                  timerStatusProhibit: tsp200,
                  timerEPC: OMIT,
                  missingPDU_Indicator: GcTRUE,
                  timerStatusPeriodic: OMIT
                }
              }
            ],
            sS_dl_RLC_Mode:
            {
              dl_PayloadSize: 128,
              dl_RLCModeInfo:
              [
                ul_AM_RLC_Mode:
                {
                  transmissionRLC_Discard:
                  [
                    noDiscard: dat15
                  ],
                  transmissionWindowSize: tw32,
                  timerRST: tr500,
                  max_RST: rst1,
                  pollingInfo:
                  {
                    timerPollProhibit: tpp200,
                    timerPoll: tp200,
                    poll_PDU: OMIT,
                    poll_SDU: sdu1,
                    lastTransmissionPDU_Poll: GcTRUE,
                    lastRetransmissionPDU_Poll: GcTRUE,
                    pollWindow: pw99,
                    timerPollPeriodic: OMIT
                  }
                }
              ]
            }
          },
          rB_LogCH_Mapping:
          {
            uLlogicalChannelIdentity: 2,
            dLlogicalChannelIdentity: 2,
            logicalChannelType: OMIT,
            cn_DomainIdentity: OMIT
          }
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 3
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          sS_rlc_Info:
          {
            sS_ul_RLC_Mode:
            [
              dl_AM_RLC_Mode:
              {
                inSequenceDelivery: GcTRUE,
                receivingWindowSize: rw32,
                dl_RLC_StatusInfo:
                {
                  timerStatusProhibit: tsp200,
                  timerEPC: OMIT,
                  missingPDU_Indicator: GcTRUE,
                  timerStatusPeriodic: OMIT
                }
              }
            ],
            sS_dl_RLC_Mode:
            {
              dl_PayloadSize: 128,
              dl_RLCModeInfo:
              [
                ul_AM_RLC_Mode:
                {
                  transmissionRLC_Discard:
                  [
                    noDiscard: dat15
                  ],
                  transmissionWindowSize: tw32,
                  timerRST: tr500,
                  max_RST: rst1,
                  pollingInfo:
                  {
                    timerPollProhibit: tpp200,
                    timerPoll: tp200,
                    poll_PDU: OMIT,
                    poll_SDU: sdu1,
                    lastTransmissionPDU_Poll: GcTRUE,
                    lastRetransmissionPDU_Poll: GcTRUE,
                    pollWindow: pw99,
                    timerPollPeriodic: OMIT
                  }
                }
              ]
            }
          },
          rB_LogCH_Mapping:
          {
            uLlogicalChannelIdentity: 3,
            dLlogicalChannelIdentity: 3,
            logicalChannelType: OMIT,
            cn_DomainIdentity: OMIT
          }
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 4
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          sS_rlc_Info:
          {
            sS_ul_RLC_Mode:
            [
              dl_AM_RLC_Mode:
              {
                inSequenceDelivery: GcTRUE,
                receivingWindowSize: rw32,
                dl_RLC_StatusInfo:
                {
                  timerStatusProhibit: tsp200,
                  timerEPC: OMIT,
                  missingPDU_Indicator: GcTRUE,
                  timerStatusPeriodic: OMIT
                }
              }
            ],
            sS_dl_RLC_Mode:
            {
              dl_PayloadSize: 128,
              dl_RLCModeInfo:
              [
                ul_AM_RLC_Mode:
                {
                  transmissionRLC_Discard:
                  [
                    noDiscard: dat15
                  ],
                  transmissionWindowSize: tw32,
                  timerRST: tr500,
                  max_RST: rst1,
                  pollingInfo:
                  {
                    timerPollProhibit: tpp200,
                    timerPoll: tp200,
                    poll_PDU: OMIT,
                    poll_SDU: sdu1,
                    lastTransmissionPDU_Poll: GcTRUE,
                    lastRetransmissionPDU_Poll: GcTRUE,
                    pollWindow: pw99,
                    timerPollPeriodic: OMIT
                  }
                }
              ]
            }
          },
          rB_LogCH_Mapping:
          {
            uLlogicalChannelIdentity: 4,
            dLlogicalChannelIdentity: 4,
            logicalChannelType: OMIT,
            cn_DomainIdentity: OMIT
          }
        }
      ]
    }

TTCN PDU: RLC_TR_DATA_IND

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        rB_Identity: 0
      ],
      tM_message:
      [
        uL_CCCH_Message: PDU:
        {
          integrityCheckInfo: OMIT,
          message:
          [
            rrcConnectionRequest:
            {
              initialUE_Identity:
              [
                tmsi_and_LAI:
                {
                  tmsi: '00010001001000100011001101000100'B,
                  lai:
                  {
                    plmn_Identity:
                    {
                      mcc:
                      [
                        0,
                        0,
                        1
                      ],
                      mnc:
                      [
                        0,
                        1
                      ]
                    },
                    lac: '0000000000000001'B
                  }
                }
              ],
              establishmentCause: registration,
              protocolErrorIndicator: noError,
              measuredResultsOnRACH: OMIT,
              v3d0NonCriticalExtensions: OMIT
            }
          ]
        }
      ]
    }

TTCN PDU: RLC_UM_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        rB_Identity: 0
      ],
      uM_message:
      [
        dL_CCCH_Message: PDU:
        {
          integrityCheckInfo: OMIT,
          message:
          [
            rrcConnectionSetup:
            [
              r3:
              {
                rrcConnectionSetup_r3:
                {
                  initialUE_Identity:
                  [
                    tmsi_and_LAI:
                    {
                      tmsi: '00010001001000100011001101000100'B,
                      lai:
                      {
                        plmn_Identity:
                        {
                          mcc:
                          [
                            0,
                            0,
                            1
                          ],
                          mnc:
                          [
                            0,
                            1
                          ]
                        },
                        lac: '0000000000000001'B
                      }
                    }
                  ],
                  rrc_TransactionIdentifier: 0,
                  activationTime: OMIT,
                  new_U_RNTI:
                  {
                    srnc_Identity: '000000000001'B,
                    s_RNTI: '00000000000000000001'B
                  },
                  new_c_RNTI: OMIT,
                  rrc_StateIndicator: cell_DCH,
                  utran_DRX_CycleLengthCoeff: 9,
                  capabilityUpdateRequirement:
                  {
                    ue_RadioCapabilityFDDUpdateRequirement: GcTRUE,
                    ue_RadioCapabilityTDDUpdateRequirement: GcFALSE,
                    systemSpecificCapUpdateReqList:
                    [
                      gsm
                    ]
                  },
                  srb_InformationSetupList:
                  [
                    {
                      rb_Identity: OMIT,
                      rlc_InfoChoice:
                      [
                        rlc_Info:
                        {
                          ul_RLC_Mode:
                          [
                            ul_UM_RLC_Mode:
                            {
                              transmissionRLC_Discard: OMIT
                            }
                          ],
                          dl_RLC_Mode:
                          [
                            dl_UM_RLC_Mode: NULL
                          ]
                        }
                      ],
                      rb_MappingInfo:
                      [
                        {
                          ul_LogicalChannelMappings:
                          [
                            oneLogicalChannel:
                            {
                              ul_TransportChannelType:
                              [
                                dch: 5
                              ],
                              logicalChannelIdentity: 1,
                              rlc_SizeList:
                              [
                                configured: NULL
                              ],
                              mac_LogicalChannelPriority: 1
                            }
                          ],
                          dl_LogicalChannelMappingList:
                          [
                            {
                              dl_TransportChannelType:
                              [
                                dch: 10
                              ],
                              logicalChannelIdentity: 1
                            }
                          ]
                        },

                        {
                          ul_LogicalChannelMappings:
                          [
                            oneLogicalChannel:
                            {
                              ul_TransportChannelType:
                              [
                                rach: NULL
                              ],
                              logicalChannelIdentity: 1,
                              rlc_SizeList:
                              [
                                explicitList:
                                [
                                  {
                                    rlc_SizeIndex: 1
                                  }
                                ]
                              ],
                              mac_LogicalChannelPriority: 1
                            }
                          ],
                          dl_LogicalChannelMappingList:
                          [
                            {
                              dl_TransportChannelType:
                              [
                                fach: NULL
                              ],
                              logicalChannelIdentity: 1
                            }
                          ]
                        }
                      ]
                    },

                    {
                      rb_Identity: OMIT,
                      rlc_InfoChoice:
                      [
                        rlc_Info:
                        {
                          ul_RLC_Mode:
                          [
                            ul_AM_RLC_Mode:
                            {
                              transmissionRLC_Discard:
                              [
                                noDiscard: dat15
                              ],
                              transmissionWindowSize: tw32,
                              timerRST: tr500,
                              max_RST: rst1,
                              pollingInfo:
                              {
                                timerPollProhibit: tpp200,
                                timerPoll: tp200,
                                poll_PDU: OMIT,
                                poll_SDU: sdu1,
                                lastTransmissionPDU_Poll: GcTRUE,
                                lastRetransmissionPDU_Poll: GcTRUE,
                                pollWindow: pw99,
                                timerPollPeriodic: OMIT
                              }
                            }
                          ],
                          dl_RLC_Mode:
                          [
                            dl_AM_RLC_Mode:
                            {
                              inSequenceDelivery: GcTRUE,
                              receivingWindowSize: rw32,
                              dl_RLC_StatusInfo:
                              {
                                timerStatusProhibit: tsp200,
                                timerEPC: OMIT,
                                missingPDU_Indicator: GcTRUE,
                                timerStatusPeriodic: OMIT
                              }
                            }
                          ]
                        }
                      ],
                      rb_MappingInfo:
                      [
                        {
                          ul_LogicalChannelMappings:
                          [
                            oneLogicalChannel:
                            {
                              ul_TransportChannelType:
                              [
                                dch: 5
                              ],
                              logicalChannelIdentity: 2,
                              rlc_SizeList:
                              [
                                configured: NULL
                              ],
                              mac_LogicalChannelPriority: 2
                            }
                          ],
                          dl_LogicalChannelMappingList:
                          [
                            {
                              dl_TransportChannelType:
                              [
                                dch: 10
                              ],
                              logicalChannelIdentity: 2
                            }
                          ]
                        },

                        {
                          ul_LogicalChannelMappings:
                          [
                            oneLogicalChannel:
                            {
                              ul_TransportChannelType:
                              [
                                rach: NULL
                              ],
                              logicalChannelIdentity: 2,
                              rlc_SizeList:
                              [
                                explicitList:
                                [
                                  {
                                    rlc_SizeIndex: 1
                                  }
                                ]
                              ],
                              mac_LogicalChannelPriority: 2
                            }
                          ],
                          dl_LogicalChannelMappingList:
                          [
                            {
                              dl_TransportChannelType:
                              [
                                fach: NULL
                              ],
                              logicalChannelIdentity: 2
                            }
                          ]
                        }
                      ]
                    },

                    {
                      rb_Identity: OMIT,
                      rlc_InfoChoice:
                      [
                        rlc_Info:
                        {
                          ul_RLC_Mode:
                          [
                            ul_AM_RLC_Mode:
                            {
                              transmissionRLC_Discard:
                              [
                                noDiscard: dat15
                              ],
                              transmissionWindowSize: tw32,
                              timerRST: tr500,
                              max_RST: rst1,
                              pollingInfo:
                              {
                                timerPollProhibit: tpp200,
                                timerPoll: tp200,
                                poll_PDU: OMIT,
                                poll_SDU: sdu1,
                                lastTransmissionPDU_Poll: GcTRUE,
                                lastRetransmissionPDU_Poll: GcTRUE,
                                pollWindow: pw99,
                                timerPollPeriodic: OMIT
                              }
                            }
                          ],
                          dl_RLC_Mode:
                          [
                            dl_AM_RLC_Mode:
                            {
                              inSequenceDelivery: GcTRUE,
                              receivingWindowSize: rw32,
                              dl_RLC_StatusInfo:
                              {
                                timerStatusProhibit: tsp200,
                                timerEPC: OMIT,
                                missingPDU_Indicator: GcTRUE,
                                timerStatusPeriodic: OMIT
                              }
                            }
                          ]
                        }
                      ],
                      rb_MappingInfo:
                      [
                        {
                          ul_LogicalChannelMappings:
                          [
                            oneLogicalChannel:
                            {
                              ul_TransportChannelType:
                              [
                                dch: 5
                              ],
                              logicalChannelIdentity: 3,
                              rlc_SizeList:
                              [
                                configured: NULL
                              ],
                              mac_LogicalChannelPriority: 3
                            }
                          ],
                          dl_LogicalChannelMappingList:
                          [
                            {
                              dl_TransportChannelType:
                              [
                                dch: 10
                              ],
                              logicalChannelIdentity: 3
                            }
                          ]
                        },

                        {
                          ul_LogicalChannelMappings:
                          [
                            oneLogicalChannel:
                            {
                              ul_TransportChannelType:
                              [
                                rach: NULL
                              ],
                              logicalChannelIdentity: 3,
                              rlc_SizeList:
                              [
                                explicitList:
                                [
                                  {
                                    rlc_SizeIndex: 1
                                  }
                                ]
                              ],
                              mac_LogicalChannelPriority: 3
                            }
                          ],
                          dl_LogicalChannelMappingList:
                          [
                            {
                              dl_TransportChannelType:
                              [
                                fach: NULL
                              ],
                              logicalChannelIdentity: 3
                            }
                          ]
                        }
                      ]
                    },

                    {
                      rb_Identity: OMIT,
                      rlc_InfoChoice:
                      [
                        rlc_Info:
                        {
                          ul_RLC_Mode:
                          [
                            ul_AM_RLC_Mode:
                            {
                              transmissionRLC_Discard:
                              [
                                noDiscard: dat15
                              ],
                              transmissionWindowSize: tw32,
                              timerRST: tr500,
                              max_RST: rst1,
                              pollingInfo:
                              {
                                timerPollProhibit: tpp200,
                                timerPoll: tp200,
                                poll_PDU: OMIT,
                                poll_SDU: sdu1,
                                lastTransmissionPDU_Poll: GcTRUE,
                                lastRetransmissionPDU_Poll: GcTRUE,
                                pollWindow: pw99,
                                timerPollPeriodic: OMIT
                              }
                            }
                          ],
                          dl_RLC_Mode:
                          [
                            dl_AM_RLC_Mode:
                            {
                              inSequenceDelivery: GcTRUE,
                              receivingWindowSize: rw32,
                              dl_RLC_StatusInfo:
                              {
                                timerStatusProhibit: tsp200,
                                timerEPC: OMIT,
                                missingPDU_Indicator: GcTRUE,
                                timerStatusPeriodic: OMIT
                              }
                            }
                          ]
                        }
                      ],
                      rb_MappingInfo:
                      [
                        {
                          ul_LogicalChannelMappings:
                          [
                            oneLogicalChannel:
                            {
                              ul_TransportChannelType:
                              [
                                dch: 5
                              ],
                              logicalChannelIdentity: 4,
                              rlc_SizeList:
                              [
                                configured: NULL
                              ],
                              mac_LogicalChannelPriority: 4
                            }
                          ],
                          dl_LogicalChannelMappingList:
                          [
                            {
                              dl_TransportChannelType:
                              [
                                dch: 10
                              ],
                              logicalChannelIdentity: 4
                            }
                          ]
                        },

                        {
                          ul_LogicalChannelMappings:
                          [
                            oneLogicalChannel:
                            {
                              ul_TransportChannelType:
                              [
                                rach: NULL
                              ],
                              logicalChannelIdentity: 4,
                              rlc_SizeList:
                              [
                                explicitList:
                                [
                                  {
                                    rlc_SizeIndex: 1
                                  }
                                ]
                              ],
                              mac_LogicalChannelPriority: 4
                            }
                          ],
                          dl_LogicalChannelMappingList:
                          [
                            {
                              dl_TransportChannelType:
                              [
                                fach: NULL
                              ],
                              logicalChannelIdentity: 4
                            }
                          ]
                        }
                      ]
                    }
                  ],
                  ul_CommonTransChInfo:
                  {
                    tfc_Subset: OMIT,
                    prach_TFCS: OMIT,
                    modeSpecificInfo:
                    [
                      fdd:
                      {
                        ul_TFCS:
                        [
                          normalTFCI_Signalling:
                          [
                            complete:
                            {
                              ctfcSize:
                              [
                                ctfc2Bit:
                                [
                                  {
                                    ctfc2: 0,
                                    powerOffsetInformation:
                                    {
                                      gainFactorInformation:
                                      [
                                        computedGainFactors: 0
                                      ],
                                      powerOffsetPp_m: OMIT
                                    }
                                  },

                                  {
                                    ctfc2: 1,
                                    powerOffsetInformation:
                                    {
                                      gainFactorInformation:
                                      [
                                        signalledGainFactors:
                                        {
                                          modeSpecificInfo:
                                          [
                                            fdd:
                                            {
                                              gainFactorBetaC: 11
                                            }
                                          ],
                                          gainFactorBetaD: 15,
                                          referenceTFC_ID: 0
                                        }
                                      ],
                                      powerOffsetPp_m: OMIT
                                    }
                                  }
                                ]
                              ]
                            }
                          ]
                        ]
                      }
                    ]
                  },
                  ul_AddReconfTransChInfoList:
                  [
                    {
                      ul_TransportChannelType: dch,
                      transportChannelIdentity: 5,
                      transportFormatSet:
                      [
                        dedicatedTransChTFS:
                        {
                          tti:
                          [
                            tti10:
                            [
                              {
                                rlc_Size:
                                [
                                  bitMode:
                                  [
                                    sizeType2:
                                    {
                                      part1: 2,
                                      part2: OMIT
                                    }
                                  ]
                                ],
                                numberOfTbSizeList:
                                [
                                  [
                                    zero: NULL
                                  ],

                                  [
                                    one: NULL
                                  ]
                                ],
                                logicalChannelList:
                                [
                                  allSizes: NULL
                                ]
                              }
                            ]
                          ],
                          semistaticTF_Information:
                          {
                            channelCodingType:
                            [
                              convolutional: third
                            ],
                            rateMatchingAttribute# 192 # crc_Size# crc16
                          }
                        }
                      ]
                    }
                  ]
                  # dl_CommonTransChInfo#
                  {
                    sccpch_TFCS# OMIT# modeSpecificInfo#
                    [
                      fdd#
                      {
                        dl_Parameters#
                        [
                          sameAsUL# NULL
                        ]
                      }
                    ]
                  }
                  # dl_AddReconfTransChInfoList#
                  [
                    {
                      dl_TransportChannelType# dch# dl_transportChannelIdentity# 10 # tfs_SignallingMode#
                      [
                        sameAsULTrCH#
                        {
                          ul_TransportChannelType# dch# ul_TransportChannelIdentity# 5
                        }
                      ]
                      # dch_QualityTarget#
                      {
                        bler_QualityValue# #20
                      }
                      # dummy# OMIT
                    }
                  ]
                  # frequencyInfo# OMIT# maxAllowedUL_TX_Power# OMIT# ul_ChannelRequirement#
                  [
                    ul_DPCH_Info#
                    {
                      ul_DPCH_PowerControlInfo#
                      [
                        fdd#
                        {
                          dpcch_PowerOffset# #40 # pc_Preamble# 1 # sRB_delay# 7 # powerControlAlgorithm#
                          [
                            algorithm1# 0
                          ]
                        }
                      ]
                      # modeSpecificInfo#
                      [
                        fdd#
                        {
                          scramblingCodeType# longSC# scramblingCode# 1000 # numberOfDPDCH# OMIT# spreadingFactor# sf64# tfci_Existence# GcTRUE # numberOfFBI_Bits# OMIT# puncturingLimit# pl1
                        }
                      ]
                    }
                  ]
                  # dl_CommonInformation#
                  {
                    dl_DPCH_InfoCommon#
                    {
                      cfnHandling#
                      [
                        initialise#
                        {
                          cfntargetsfnframeoffset# OMIT
                        }
                      ]
                      # modeSpecificInfo#
                      [
                        fdd#
                        {
                          dl_DPCH_PowerControlInfo#
                          {
                            modeSpecificInfo#
                            [
                              fdd#
                              {
                                dpc_Mode# singleTPC
                              }
                            ]
                          }
                          # powerOffsetPilot_pdpdch# 0 # dl_rate_matching_restriction# OMIT# spreadingFactorAndPilot#
                          [
                            sfd128# pb4
                          ]
                          # positionFixedOrFlexible# fixed# tfci_Existence# GcFALSE
                        }
                      ]
                    }
                    # modeSpecificInfo#
                    [
                      fdd#
                      {
                        defaultDPCH_OffsetValue# 0 # dpch_CompressedModeInfo# OMIT# tx_DiversityMode# noDiversity# ssdt_Information# OMIT
                      }
                    ]
                  }
                  # dl_InformationPerRL_List#
                  [
                    {
                      modeSpecificInfo#
                      [
                        fdd#
                        {
                          primaryCPICH_Info#
                          {
                            primaryScramblingCode# 150
                          }
                          # pdsch_SHO_DCH_Info# OMIT# pdsch_CodeMapping# OMIT
                        }
                      ]
                      # dl_DPCH_InfoPerRL#
                      [
                        fdd#
                        {
                          pCPICH_UsageForChannelEst# mayBeUsed# dpch_FrameOffset# 0 # secondaryCPICH_Info# OMIT# dl_ChannelisationCodeList#
                          [
                            {
                              secondaryScramblingCode# 1 # sf_AndCodeNumber#
                              [
                                sf128# 0
                              ]
                              # scramblingCodeChange# noCodeChange
                            }
                          ]
                          # tpc_CombinationIndex# 0 # ssdt_CellIdentity# OMIT# closedLoopTimingAdjMode# OMIT
                        }
                      ]
                      # sccpch_InfoforFACH# OMIT
                    }
                  ]
                }
                # laterNonCriticalExtensions# OMIT
              }
            ]
          ]
        }
      ]
      # specialLI# GcTRUE
    }

TTCN PDU: RLC_AM_DATA_IND

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 2
      ],
      integrityResult:
      [
        integrityUsed: i_pass
      ],
      aM_message:
      [
        uL_DCCH_Message: PDU:
        {
          integrityCheckInfo: OMIT,
          message:
          [
            rrcConnectionSetupComplete:
            {
              rrc_TransactionIdentifier: 0,
              startList:
              [
                {
                  cn_DomainIdentity: ps_domain,
                  start_Value: '00000000000000000010'B
                },

                {
                  cn_DomainIdentity: cs_domain,
                  start_Value: '00000000000000000010'B
                }
              ],
              ue_RadioAccessCapability:
              {
                accessStratumReleaseIndicator: r99,
                pdcp_Capability:
                {
                  losslessSRNS_RelocationSupport: GcFALSE,
                  supportForRfc2507:
                  [
                    notSupported: NULL
                  ]
                },
                rlc_Capability:
                {
                  totalRLC_AM_BufferSize: kb50,
                  maximumRLC_WindowSize: mws2047,
                  maximumAM_EntityNumber: am6
                },
                transportChannelCapability:
                {
                  dl_TransChCapability:
                  {
                    maxNoBitsReceived: b8960,
                    maxConvCodeBitsReceived: b1280,
                    turboDecodingSupport:
                    [
                      supported: b8960
                    ],
                    maxSimultaneousTransChs: e8,
                    maxSimultaneousCCTrCH_Count: 1,
                    maxReceivedTransportBlocks: tb32,
                    maxNumberOfTFC: tfc128,
                    maxNumberOfTF: tf64
                  },
                  ul_TransChCapability:
                  {
                    maxNoBitsTransmitted: b3840,
                    maxConvCodeBitsTransmitted: b1280,
                    turboEncodingSupport:
                    [
                      supported: b3840
                    ],
                    maxSimultaneousTransChs: e8,
                    modeSpecificInfo:
                    [
                      fdd: NULL
                    ],
                    maxTransmittedBlocks: tb32,
                    maxNumberOfTFC: tfc64,
                    maxNumberOfTF: tf32
                  }
                },
                rf_Capability:
                {
                  fddRF_Capability:
                  {
                    ue_PowerClass: 4,
                    txRxFrequencySeparation: mhz190
                  },
                  tddRF_Capability: OMIT
                },
                physicalChannelCapability:
                {
                  fddPhysChCapability:
                  {
                    downlinkPhysChCapability:
                    {
                      maxNoDPCH_PDSCH_Codes: 1,
                      maxNoPhysChBitsReceived: b9600,
                      supportForSF_512: GcFALSE,
                      supportOfPDSCH: GcFALSE,
                      simultaneousSCCPCH_DPCH_Reception:
                      [
                        notSupported: NULL
                      ]
                    },
                    uplinkPhysChCapability:
                    {
                      maxNoDPDCH_BitsTransmitted: b4800,
                      supportOfPCPCH: GcFALSE
                    }
                  },
                  tddPhysChCapability: OMIT
                },
                ue_MultiModeRAT_Capability:
                {
                  multiRAT_CapabilityList:
                  {
                    supportOfGSM: GcFALSE,
                    supportOfMulticarrier: GcFALSE
                  },
                  multiModeCapability: fdd
                },
                securityCapability:
                {
                  cipheringAlgorithmCap: '0000000000000011'B,
                  integrityProtectionAlgorithmCap: '0000000000000010'B
                },
                ue_positioning_Capability:
                {
                  standaloneLocMethodsSupported: GcFALSE,
                  ue_BasedOTDOA_Supported: GcFALSE,
                  networkAssistedGPS_Supported: noNetworkAssistedGPS,
                  supportForUE_GPS_TimingOfCellFrames: GcFALSE,
                  supportForIPDL: GcFALSE
                },
                measurementCapability:
                {
                  downlinkCompressedMode:
                  {
                    fdd_Measurements: GcTRUE,
                    tdd_Measurements: OMIT,
                    gsm_Measurements:
                    {
                      gsm900: GcTRUE,
                      dcs1800: GcTRUE,
                      gsm1900: GcTRUE
                    },
                    multiCarrierMeasurements: GcFALSE
                  },
                  uplinkCompressedMode:
                  {
                    fdd_Measurements: GcTRUE,
                    tdd_Measurements: OMIT,
                    gsm_Measurements:
                    {
                      gsm900: GcTRUE,
                      dcs1800: GcTRUE,
                      gsm1900: GcTRUE
                    },
                    multiCarrierMeasurements: GcFALSE
                  }
                }
              },
              ue_RATSpecificCapability: OMIT,
              v370NonCriticalExtensions: OMIT
            }
          ]
        }
      ]
    }

TTCN PDU: RRC_DataInd

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      rB_Id: 3,
      ch: OMIT,
      sapId: OMIT,
      cN_Domain: 1,
      start: '00000000000000000010'B,
      msg: PDU:
      {
        skipIndicator: '0000'B,
        gMMProtocolDiscriminator: '1000'B,
        msgType: '00001000'B,
        gprsCiphKeySeqNo:
        {
          spare1: '0'B,
          keySeq: '001'B
        },
        updateType:
        {
          for: '0'B,
          value: '000'B
        },
        oldRAI:
        {
          plmn: '00F110'O,
          lac: '0001'O,
          rac: '05'O
        },
        msRadioAccessCap:
        {
          iel: '0B'O,
          value: '15F38233542A332644A198'O
        },
        oldPTMSI_Signature: OMIT,
        readyTimer:
        {
          iei: '00010111'B,
          unit: '000'B,
          value: '10110'B
        },
        drxParameter:
        {
          iei: '00100111'B,
          splitPGcycleCode: '00000111'B,
          cnDRXcoef: '0000'B,
          splitOnCCCH: '0'B,
          nonDRXtimer: '100'B
        },
        tmsiStatus: OMIT,
        ptmsi:
        {
          iei: '00011000'B,
          iel: '05'O,
          iDigit1: '1111'B,
          oddEvenInd: '0'B,
          typeOfId: '100'B,
          otherDigits: '12345678'O
        },
        msnetworkcap:
        {
          iei: '00110001'B,
          iel: '02'O,
          value: 'E540'O
        },
        pDP_ContextStatus:
        {
          iei: '00110010'B,
          iel: '02'O,
          nSAPI: '0000000000000000'B
        }
      }
    }

TTCN PDU: RRC_DataReq

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      rB_Id: 3,
      ch: OMIT,
      sapId: OMIT,
      cN_Domain: 1,
      msg: PDU:
      {
        skipIndicator: '0000'B,
        gMMProtocolDiscriminator: '1000'B,
        msgType: '00001011'B,
        gmmCause: '03'O,
        spare: '0000'B,
        forceToStandby:
        {
          spare: '0'B,
          value: '000'B
        },
        t3302Value: OMIT
      }
    }

TTCN PDU: RLC_UM_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 1
      ],
      uM_message:
      [
        dL_DCCH_Message: PDU:
        {
          integrityCheckInfo: OMIT,
          message:
          [
            rrcConnectionRelease:
            [
              r3:
              {
                rrcConnectionRelease_r3:
                {
                  rrc_TransactionIdentifier: 0,
                  n_308: 1,
                  releaseCause: normalEvent,
                  rplmn_information: OMIT
                },
                laterNonCriticalExtensions: OMIT
              }
            ]
          ]
        }
      ],
      specialLI: GcFALSE
    }

TTCN PDU: RLC_UM_DATA_IND

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 1
      ],
      integrityResult:
      [
        integrityUsed: i_pass
      ],
      uM_message:
      [
        uL_DCCH_Message: PDU:
        {
          integrityCheckInfo: OMIT,
          message:
          [
            rrcConnectionReleaseComplete:
            {
              rrc_TransactionIdentifier: 0,
              errorIndication: OMIT,
              laterNonCriticalExtensions: OMIT
            }
          ]
        }
      ]
    }

TTCN PDU: RLC_UM_DATA_IND

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 1
      ],
      integrityResult:
      [
        integrityUsed: i_pass
      ],
      uM_message:
      [
        uL_DCCH_Message: PDU:
        {
          integrityCheckInfo: OMIT,
          message:
          [
            rrcConnectionReleaseComplete:
            {
              rrc_TransactionIdentifier: 0,
              errorIndication: OMIT,
              laterNonCriticalExtensions: OMIT
            }
          ]
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 1
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 2
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 3
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 4
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 1
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          sS_rlc_Info:
          {
            sS_ul_RLC_Mode:
            [
              dl_UM_RLC_Mode: NULL
            ],
            sS_dl_RLC_Mode:
            {
              dl_PayloadSize: 136,
              dl_RLCModeInfo:
              [
                ul_UM_RLC_Mode:
                {
                  transmissionRLC_Discard:
                  [
                    timerBasedNoExplicit: dt100
                  ]
                }
              ]
            }
          },
          rB_LogCH_Mapping:
          {
            uLlogicalChannelIdentity: 1,
            dLlogicalChannelIdentity: 1,
            logicalChannelType: OMIT,
            cn_DomainIdentity: OMIT
          }
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 2
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          sS_rlc_Info:
          {
            sS_ul_RLC_Mode:
            [
              dl_AM_RLC_Mode:
              {
                inSequenceDelivery: GcTRUE,
                receivingWindowSize: rw32,
                dl_RLC_StatusInfo:
                {
                  timerStatusProhibit: tsp200,
                  timerEPC: OMIT,
                  missingPDU_Indicator: GcTRUE,
                  timerStatusPeriodic: OMIT
                }
              }
            ],
            sS_dl_RLC_Mode:
            {
              dl_PayloadSize: 128,
              dl_RLCModeInfo:
              [
                ul_AM_RLC_Mode:
                {
                  transmissionRLC_Discard:
                  [
                    noDiscard: dat15
                  ],
                  transmissionWindowSize: tw32,
                  timerRST: tr500,
                  max_RST: rst1,
                  pollingInfo:
                  {
                    timerPollProhibit: tpp200,
                    timerPoll: tp200,
                    poll_PDU: OMIT,
                    poll_SDU: sdu1,
                    lastTransmissionPDU_Poll: GcTRUE,
                    lastRetransmissionPDU_Poll: GcTRUE,
                    pollWindow: pw99,
                    timerPollPeriodic: OMIT
                  }
                }
              ]
            }
          },
          rB_LogCH_Mapping:
          {
            uLlogicalChannelIdentity: 2,
            dLlogicalChannelIdentity: 2,
            logicalChannelType: OMIT,
            cn_DomainIdentity: OMIT
          }
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 3
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          sS_rlc_Info:
          {
            sS_ul_RLC_Mode:
            [
              dl_AM_RLC_Mode:
              {
                inSequenceDelivery: GcTRUE,
                receivingWindowSize: rw32,
                dl_RLC_StatusInfo:
                {
                  timerStatusProhibit: tsp200,
                  timerEPC: OMIT,
                  missingPDU_Indicator: GcTRUE,
                  timerStatusPeriodic: OMIT
                }
              }
            ],
            sS_dl_RLC_Mode:
            {
              dl_PayloadSize: 128,
              dl_RLCModeInfo:
              [
                ul_AM_RLC_Mode:
                {
                  transmissionRLC_Discard:
                  [
                    noDiscard: dat15
                  ],
                  transmissionWindowSize: tw32,
                  timerRST: tr500,
                  max_RST: rst1,
                  pollingInfo:
                  {
                    timerPollProhibit: tpp200,
                    timerPoll: tp200,
                    poll_PDU: OMIT,
                    poll_SDU: sdu1,
                    lastTransmissionPDU_Poll: GcTRUE,
                    lastRetransmissionPDU_Poll: GcTRUE,
                    pollWindow: pw99,
                    timerPollPeriodic: OMIT
                  }
                }
              ]
            }
          },
          rB_LogCH_Mapping:
          {
            uLlogicalChannelIdentity: 3,
            dLlogicalChannelIdentity: 3,
            logicalChannelType: OMIT,
            cn_DomainIdentity: OMIT
          }
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 4
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          sS_rlc_Info:
          {
            sS_ul_RLC_Mode:
            [
              dl_AM_RLC_Mode:
              {
                inSequenceDelivery: GcTRUE,
                receivingWindowSize: rw32,
                dl_RLC_StatusInfo:
                {
                  timerStatusProhibit: tsp200,
                  timerEPC: OMIT,
                  missingPDU_Indicator: GcTRUE,
                  timerStatusPeriodic: OMIT
                }
              }
            ],
            sS_dl_RLC_Mode:
            {
              dl_PayloadSize: 128,
              dl_RLCModeInfo:
              [
                ul_AM_RLC_Mode:
                {
                  transmissionRLC_Discard:
                  [
                    noDiscard: dat15
                  ],
                  transmissionWindowSize: tw32,
                  timerRST: tr500,
                  max_RST: rst1,
                  pollingInfo:
                  {
                    timerPollProhibit: tpp200,
                    timerPoll: tp200,
                    poll_PDU: OMIT,
                    poll_SDU: sdu1,
                    lastTransmissionPDU_Poll: GcTRUE,
                    lastRetransmissionPDU_Poll: GcTRUE,
                    pollWindow: pw99,
                    timerPollPeriodic: OMIT
                  }
                }
              ]
            }
          },
          rB_LogCH_Mapping:
          {
            uLlogicalChannelIdentity: 4,
            dLlogicalChannelIdentity: 4,
            logicalChannelType: OMIT,
            cn_DomainIdentity: OMIT
          }
        }
      ]
    }

TTCN PDU: CMAC_PAGING_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        physicalChannelIdentity: 5
      ],
      ratType: fdd,
      configMessage:
      {
        pI_BitMapInfo:
        [
          e18: '000000000000000100'B
        ],
        dRX_CycleLength: 7,
        iMSI:
        [
          0,
          0,
          1,
          0,
          1,
          0,
          0,
          0,
          0,
          0,
          0,
          0,
          3,
          3,
          3
        ],
        t_pich_T_sccpch: GcFALSE
      }
    }

TTCN PDU: CMAC_PAGING_Config_CNF

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        physicalChannelIdentity: 5
      ]
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        rB_Identity: -2
      ],
      tM_message:
      [
        pCCH_Message: PDU:
        {
          message:
          [
            pagingType1:
            {
              pagingRecordList:
              [
                [
                  cn_Identity:
                  {
                    pagingCause: terminatingInteractiveCall,
                    cn_DomainIdentity: ps_domain,
                    cn_pagedUE_Identity:
                    [
                      p_TMSI_GSM_MAP: '00010010001101000101011001111000'B
                    ]
                  }
                ]
              ],
              bcch_ModificationInfo: OMIT,
              laterNonCriticalExtensions: OMIT
            }
          ]
        }
      ]
    }

TTCN PDU: CPHY_Cell_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      tcell: 321,
      sfnOffset: 3000,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10837
          }
        ]
      },
      primaryScramblingCode_SS: 250,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      dLTxAttenuationLevel: 0
    }

TTCN PDU: CPHY_RL_Setup_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        physicalChannelIdentity: 0
      ],
      ratType: fdd,
      setupMessage:
      {
        physicalChannelInfo:
        [
          primaryCPICHInfo:
          {
            dl_TxPower_PCPICH: -60,
            txdiversityIndicator: GcFALSE
          }
        ]
      }
    }

TTCN PDU: CPHY_RL_Setup_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        physicalChannelIdentity: 1
      ],
      ratType: fdd,
      setupMessage:
      {
        physicalChannelInfo:
        [
          primarySCHInfo:
          {
            tstdIndicator: GcFALSE,
            dl_TxPower: -5
          }
        ]
      }
    }

TTCN PDU: CPHY_RL_Setup_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        physicalChannelIdentity: 2
      ],
      ratType: fdd,
      setupMessage:
      {
        physicalChannelInfo:
        [
          secondarySCHInfo:
          {
            tstdIndicator: GcFALSE,
            dl_TxPower: -5
          }
        ]
      }
    }

TTCN PDU: CPHY_RL_Setup_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        physicalChannelIdentity: 4
      ],
      ratType: fdd,
      setupMessage:
      {
        physicalChannelInfo:
        [
          primaryCCPCHInfo:
          {
            sttd_Indicator: GcFALSE,
            dl_TxPower: -2
          }
        ]
      }
    }

TTCN PDU: CPHY_TrCH_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        physicalChannelIdentity: 4
      ],
      ratType: fdd,
      trchConfigType:
      [
        nonDch: NULL
      ],
      configMessage:
      {
        activationTime:
        [
          activateNow: NULL
        ],
        ulconnectedTrCHList: OMIT,
        ulTFCS: OMIT,
        dlconnectedTrCHList:
        [
          {
            trchid: 11,
            dl_TransportChannelType: bch,
            transportChannelInfo:
            {
              tti:
              [
                tti20:
                [
                  {
                    tb_Size: 246,
                    numberOfTbSizeList:
                    [
                      [
                        one: NULL
                      ]
                    ],
                    logicalChannelList:
                    [
                      configured: NULL
                    ]
                  }
                ]
              ],
              semistaticTF_Information:
              {
                channelCodingType:
                [
                  convolutional: half
                ],
                rateMatchingAttribute# 1 # crc_Size# crc16
              }
            }
          }
        ]
        # dlTFCS#
        [
          normalTFCI_Signalling#
          [
            complete#
            {
              ctfcSize#
              [
                ctfc2Bit#
                [
                  {
                    ctfc2# 0 # powerOffsetInformation#
                    {
                      gainFactorInformation#
                      [
                        signalledGainFactors#
                        {
                          modeSpecificInfo#
                          [
                            fdd#
                            {
                              gainFactorBetaC# 11
                            }
                          ]
                          # gainFactorBetaD# 15 # referenceTFC_ID# 0
                        }
                      ]
                      # powerOffsetPp_m# OMIT
                    }
                  }
                ]
              ]
            }
          ]
        ]
      }
    }

TTCN PDU: CPHY_TrCH_Config_CNF

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        physicalChannelIdentity: 4
      ]
    }

TTCN PDU: CMAC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        physicalChannelIdentity: 4
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          activationTime:
          [
            activateNow: NULL
          ],
          uE_Info:
          {
            u_RNTI: OMIT,
            c_RNTI: OMIT
          },
          trCHInfo:
          {
            ulconnectedTrCHList: OMIT,
            ulTFCS: OMIT,
            dlconnectedTrCHList:
            [
              {
                trchid: 11,
                transportChannelInfo:
                {
                  tti:
                  [
                    tti20:
                    [
                      {
                        tb_Size: 246,
                        numberOfTbSizeList:
                        [
                          [
                            one: NULL
                          ]
                        ],
                        logicalChannelList:
                        [
                          configured: NULL
                        ]
                      }
                    ]
                  ],
                  semistaticTF_Information:
                  {
                    channelCodingType:
                    [
                      convolutional: half
                    ],
                    rateMatchingAttribute# 1 # crc_Size# crc16
                  }
                }
              }
            ]
            # dlTFCS#
            [
              normalTFCI_Signalling#
              [
                complete#
                {
                  ctfcSize#
                  [
                    ctfc2Bit#
                    [
                      {
                        ctfc2# 0 # powerOffsetInformation#
                        {
                          gainFactorInformation#
                          [
                            signalledGainFactors#
                            {
                              modeSpecificInfo#
                              [
                                fdd#
                                {
                                  gainFactorBetaC# 11
                                }
                              ]
                              # gainFactorBetaD# 15 # referenceTFC_ID# 0
                            }
                          ]
                          # powerOffsetPp_m# OMIT
                        }
                      }
                    ]
                  ]
                }
              ]
            ]
          }
          # trCH_LogCHMapping#
          {
            ulconnectedTrCHList# OMIT# dlconnectedTrCHList#
            [
              {
                trchid# 11 # trCH_LogCHMappingList#
                [
                  {
                    logicalChannel_Mapping#
                    [
                      dl_LogicalChannelMapping#
                      {
                        macHeaderManipulation# normalMacHeader# dl_TransportChannelType# bch# logicalChannelIdentity# 1 # logicalChannelType# bCCH# rlc_SizeList#
                        [
                          configured# NULL
                        ]
                        # mac_LogicalChannelPriority# 1
                      }
                    ]
                    # rB_Identity# #1 # cn_DomainIdentity# OMIT
                  }
                ]
              }
            ]
          }
        }
      ]
    }

TTCN PDU: CPHY_RL_Setup_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        physicalChannelIdentity: 5
      ],
      ratType: fdd,
      setupMessage:
      {
        physicalChannelInfo:
        [
          secondaryCCPCHInfo:
          {
            scramblingCode: 0,
            dl_ChannelizationCode:
            [
              sf64: 1
            ],
            sCCPCHSlotFormat: 8,
            timingOffset: 0,
            positionFixedOrFlexible: flexible,
            sttd_Indicator: GcFALSE,
            dl_TxPower: -2,
            powerOffsetOfTFCI_PO1: 6,
            powerOffsetOfPILOT_PO3: 6
          }
        ]
      }
    }

TTCN PDU: CPHY_TrCH_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        physicalChannelIdentity: 5
      ],
      ratType: fdd,
      trchConfigType:
      [
        nonDch: NULL
      ],
      configMessage:
      {
        activationTime:
        [
          activateNow: NULL
        ],
        ulconnectedTrCHList: OMIT,
        ulTFCS: OMIT,
        dlconnectedTrCHList:
        [
          {
            trchid: 12,
            dl_TransportChannelType: pch,
            transportChannelInfo:
            {
              tti:
              [
                tti10:
                [
                  {
                    tb_Size: 240,
                    numberOfTbSizeList:
                    [
                      [
                        zero: NULL
                      ],

                      [
                        one: NULL
                      ]
                    ],
                    logicalChannelList:
                    [
                      allSizes: NULL
                    ]
                  }
                ]
              ],
              semistaticTF_Information:
              {
                channelCodingType:
                [
                  convolutional: half
                ],
                rateMatchingAttribute# 230 # crc_Size# crc16
              }
            }
          }
          #
          {
            trchid# 13 # dl_TransportChannelType# fach# transportChannelInfo#
            {
              tti#
              [
                tti10#
                [
                  {
                    tb_Size# 168 # numberOfTbSizeList#
                    [
                      [
                        zero# NULL
                      ]
                      #
                      [
                        one# NULL
                      ]
                      #
                      [
                        small# 2
                      ]
                    ]
                    # logicalChannelList#
                    [
                      allSizes# NULL
                    ]
                  }
                ]
              ]
              # semistaticTF_Information#
              {
                channelCodingType#
                [
                  convolutional# half
                ]
                # rateMatchingAttribute# 220 # crc_Size# crc16
              }
            }
          }
          #
          {
            trchid# 14 # dl_TransportChannelType# fach# transportChannelInfo#
            {
              tti#
              [
                tti10#
                [
                  {
                    tb_Size# 360 # numberOfTbSizeList#
                    [
                      [
                        zero# NULL
                      ]
                      #
                      [
                        one# NULL
                      ]
                    ]
                    # logicalChannelList#
                    [
                      allSizes# NULL
                    ]
                  }
                ]
              ]
              # semistaticTF_Information#
              {
                channelCodingType#
                [
                  turbo# NULL
                ]
                # rateMatchingAttribute# 130 # crc_Size# crc16
              }
            }
          }
        ]
        # dlTFCS#
        [
          normalTFCI_Signalling#
          [
            complete#
            {
              ctfcSize#
              [
                ctfc4Bit#
                [
                  {
                    ctfc4# 0 # powerOffsetInformation#
                    {
                      gainFactorInformation#
                      [
                        computedGainFactors# 0
                      ]
                      # powerOffsetPp_m# OMIT
                    }
                  }
                  #
                  {
                    ctfc4# 1 # powerOffsetInformation#
                    {
                      gainFactorInformation#
                      [
                        computedGainFactors# 0
                      ]
                      # powerOffsetPp_m# OMIT
                    }
                  }
                  #
                  {
                    ctfc4# 2 # powerOffsetInformation#
                    {
                      gainFactorInformation#
                      [
                        computedGainFactors# 0
                      ]
                      # powerOffsetPp_m# OMIT
                    }
                  }
                  #
                  {
                    ctfc4# 3 # powerOffsetInformation#
                    {
                      gainFactorInformation#
                      [
                        computedGainFactors# 0
                      ]
                      # powerOffsetPp_m# OMIT
                    }
                  }
                  #
                  {
                    ctfc4# 4 # powerOffsetInformation#
                    {
                      gainFactorInformation#
                      [
                        computedGainFactors# 0
                      ]
                      # powerOffsetPp_m# OMIT
                    }
                  }
                  #
                  {
                    ctfc4# 5 # powerOffsetInformation#
                    {
                      gainFactorInformation#
                      [
                        computedGainFactors# 0
                      ]
                      # powerOffsetPp_m# OMIT
                    }
                  }
                  #
                  {
                    ctfc4# 6 # powerOffsetInformation#
                    {
                      gainFactorInformation#
                      [
                        computedGainFactors# 0
                      ]
                      # powerOffsetPp_m# OMIT
                    }
                  }
                  #
                  {
                    ctfc4# 8 # powerOffsetInformation#
                    {
                      gainFactorInformation#
                      [
                        signalledGainFactors#
                        {
                          modeSpecificInfo#
                          [
                            fdd#
                            {
                              gainFactorBetaC# 11
                            }
                          ]
                          # gainFactorBetaD# 15 # referenceTFC_ID# 0
                        }
                      ]
                      # powerOffsetPp_m# OMIT
                    }
                  }
                ]
              ]
            }
          ]
        ]
      }
    }

TTCN PDU: CMAC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        physicalChannelIdentity: 5
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          activationTime:
          [
            activateNow: NULL
          ],
          uE_Info:
          {
            u_RNTI: OMIT,
            c_RNTI: OMIT
          },
          trCHInfo:
          {
            ulconnectedTrCHList: OMIT,
            ulTFCS: OMIT,
            dlconnectedTrCHList:
            [
              {
                trchid: 12,
                transportChannelInfo:
                {
                  tti:
                  [
                    tti10:
                    [
                      {
                        tb_Size: 240,
                        numberOfTbSizeList:
                        [
                          [
                            zero: NULL
                          ],

                          [
                            one: NULL
                          ]
                        ],
                        logicalChannelList:
                        [
                          allSizes: NULL
                        ]
                      }
                    ]
                  ],
                  semistaticTF_Information:
                  {
                    channelCodingType:
                    [
                      convolutional: half
                    ],
                    rateMatchingAttribute# 230 # crc_Size# crc16
                  }
                }
              }
              #
              {
                trchid# 13 # transportChannelInfo#
                {
                  tti#
                  [
                    tti10#
                    [
                      {
                        tb_Size# 168 # numberOfTbSizeList#
                        [
                          [
                            zero# NULL
                          ]
                          #
                          [
                            one# NULL
                          ]
                          #
                          [
                            small# 2
                          ]
                        ]
                        # logicalChannelList#
                        [
                          allSizes# NULL
                        ]
                      }
                    ]
                  ]
                  # semistaticTF_Information#
                  {
                    channelCodingType#
                    [
                      convolutional# half
                    ]
                    # rateMatchingAttribute# 220 # crc_Size# crc16
                  }
                }
              }
              #
              {
                trchid# 14 # transportChannelInfo#
                {
                  tti#
                  [
                    tti10#
                    [
                      {
                        tb_Size# 360 # numberOfTbSizeList#
                        [
                          [
                            zero# NULL
                          ]
                          #
                          [
                            one# NULL
                          ]
                        ]
                        # logicalChannelList#
                        [
                          allSizes# NULL
                        ]
                      }
                    ]
                  ]
                  # semistaticTF_Information#
                  {
                    channelCodingType#
                    [
                      turbo# NULL
                    ]
                    # rateMatchingAttribute# 130 # crc_Size# crc16
                  }
                }
              }
            ]
            # dlTFCS#
            [
              normalTFCI_Signalling#
              [
                complete#
                {
                  ctfcSize#
                  [
                    ctfc4Bit#
                    [
                      {
                        ctfc4# 0 # powerOffsetInformation#
                        {
                          gainFactorInformation#
                          [
                            computedGainFactors# 0
                          ]
                          # powerOffsetPp_m# OMIT
                        }
                      }
                      #
                      {
                        ctfc4# 1 # powerOffsetInformation#
                        {
                          gainFactorInformation#
                          [
                            computedGainFactors# 0
                          ]
                          # powerOffsetPp_m# OMIT
                        }
                      }
                      #
                      {
                        ctfc4# 2 # powerOffsetInformation#
                        {
                          gainFactorInformation#
                          [
                            computedGainFactors# 0
                          ]
                          # powerOffsetPp_m# OMIT
                        }
                      }
                      #
                      {
                        ctfc4# 3 # powerOffsetInformation#
                        {
                          gainFactorInformation#
                          [
                            computedGainFactors# 0
                          ]
                          # powerOffsetPp_m# OMIT
                        }
                      }
                      #
                      {
                        ctfc4# 4 # powerOffsetInformation#
                        {
                          gainFactorInformation#
                          [
                            computedGainFactors# 0
                          ]
                          # powerOffsetPp_m# OMIT
                        }
                      }
                      #
                      {
                        ctfc4# 5 # powerOffsetInformation#
                        {
                          gainFactorInformation#
                          [
                            computedGainFactors# 0
                          ]
                          # powerOffsetPp_m# OMIT
                        }
                      }
                      #
                      {
                        ctfc4# 6 # powerOffsetInformation#
                        {
                          gainFactorInformation#
                          [
                            computedGainFactors# 0
                          ]
                          # powerOffsetPp_m# OMIT
                        }
                      }
                      #
                      {
                        ctfc4# 8 # powerOffsetInformation#
                        {
                          gainFactorInformation#
                          [
                            signalledGainFactors#
                            {
                              modeSpecificInfo#
                              [
                                fdd#
                                {
                                  gainFactorBetaC# 11
                                }
                              ]
                              # gainFactorBetaD# 15 # referenceTFC_ID# 0
                            }
                          ]
                          # powerOffsetPp_m# OMIT
                        }
                      }
                    ]
                  ]
                }
              ]
            ]
          }
          # trCH_LogCHMapping#
          {
            ulconnectedTrCHList# OMIT# dlconnectedTrCHList#
            [
              {
                trchid# 12 # trCH_LogCHMappingList#
                [
                  {
                    logicalChannel_Mapping#
                    [
                      dl_LogicalChannelMapping#
                      {
                        macHeaderManipulation# normalMacHeader# dl_TransportChannelType# pch# logicalChannelIdentity# 1 # logicalChannelType# pCCH# rlc_SizeList#
                        [
                          configured# NULL
                        ]
                        # mac_LogicalChannelPriority# 1
                      }
                    ]
                    # rB_Identity# #2 # cn_DomainIdentity# OMIT
                  }
                ]
              }
              #
              {
                trchid# 13 # trCH_LogCHMappingList#
                [
                  {
                    logicalChannel_Mapping#
                    [
                      dl_LogicalChannelMapping#
                      {
                        macHeaderManipulation# normalMacHeader# dl_TransportChannelType# fach# logicalChannelIdentity# 5 # logicalChannelType# cCCH# rlc_SizeList#
                        [
                          configured# NULL
                        ]
                        # mac_LogicalChannelPriority# 1
                      }
                    ]
                    # rB_Identity# 0 # cn_DomainIdentity# OMIT
                  }
                ]
              }
            ]
          }
        }
      ]
    }

TTCN PDU: CPHY_RL_Setup_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        physicalChannelIdentity: 6
      ],
      ratType: fdd,
      setupMessage:
      {
        physicalChannelInfo:
        [
          pICHInfo:
          {
            pichinfo:
            [
              fdd:
              {
                channelisationCode256: 2,
                pi_CountPerFrame: e18,
                sttd_Indicator: GcFALSE
              }
            ],
            dl_TxPower: -5,
            sccpchId_associated: 5
          }
        ]
      }
    }

TTCN PDU: CPHY_RL_Setup_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        physicalChannelIdentity: 7
      ],
      ratType: fdd,
      setupMessage:
      {
        physicalChannelInfo:
        [
          aICHInfo:
          {
            aichinfo:
            {
              channelisationCode256: 3,
              sttd_Indicator: GcFALSE,
              aich_TransmissionTiming: e0
            },
            dl_TxPower: -5
          }
        ]
      }
    }

TTCN PDU: CPHY_RL_Setup_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        physicalChannelIdentity: 8
      ],
      ratType: fdd,
      setupMessage:
      {
        physicalChannelInfo:
        [
          pRACHInfo:
          {
            fdd_tdd:
            [
              fdd:
              {
                preambleSignature: '0000000011111111'B,
                spreadingFactorForDataPart: sfpr64,
                preambleScramblingCode: 0,
                puncturingLimit: pl1,
                accessSlot: '111111111111'B
              }
            ]
          }
        ]
      }
    }

TTCN PDU: CPHY_TrCH_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        physicalChannelIdentity: 8
      ],
      ratType: fdd,
      trchConfigType:
      [
        nonDch: NULL
      ],
      configMessage:
      {
        activationTime:
        [
          activateNow: NULL
        ],
        ulconnectedTrCHList:
        [
          {
            trchid: 15,
            ul_TransportChannelType: rach,
            transportChannelInfo:
            {
              tti:
              [
                tti20:
                [
                  {
                    tb_Size: 168,
                    numberOfTbSizeList:
                    [
                      [
                        one: NULL
                      ]
                    ],
                    logicalChannelList:
                    [
                      configured: NULL
                    ]
                  },

                  {
                    tb_Size: 360,
                    numberOfTbSizeList:
                    [
                      [
                        one: NULL
                      ]
                    ],
                    logicalChannelList:
                    [
                      configured: NULL
                    ]
                  }
                ]
              ],
              semistaticTF_Information:
              {
                channelCodingType:
                [
                  convolutional: half
                ],
                rateMatchingAttribute# 150 # crc_Size# crc16
              }
            }
          }
        ]
        # ulTFCS#
        [
          normalTFCI_Signalling#
          [
            complete#
            {
              ctfcSize#
              [
                ctfc2Bit#
                [
                  {
                    ctfc2# 0 # powerOffsetInformation# OMIT
                  }
                  #
                  {
                    ctfc2# 1 # powerOffsetInformation# OMIT
                  }
                ]
              ]
            }
          ]
        ]
        # dlconnectedTrCHList# OMIT# dlTFCS# OMIT
      }
    }

TTCN PDU: CMAC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        physicalChannelIdentity: 8
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          activationTime:
          [
            activateNow: NULL
          ],
          uE_Info:
          {
            u_RNTI: OMIT,
            c_RNTI: OMIT
          },
          trCHInfo:
          {
            ulconnectedTrCHList:
            [
              {
                trchid: 15,
                transportChannelInfo:
                {
                  tti:
                  [
                    tti20:
                    [
                      {
                        tb_Size: 168,
                        numberOfTbSizeList:
                        [
                          [
                            one: NULL
                          ]
                        ],
                        logicalChannelList:
                        [
                          configured: NULL
                        ]
                      },

                      {
                        tb_Size: 360,
                        numberOfTbSizeList:
                        [
                          [
                            one: NULL
                          ]
                        ],
                        logicalChannelList:
                        [
                          configured: NULL
                        ]
                      }
                    ]
                  ],
                  semistaticTF_Information:
                  {
                    channelCodingType:
                    [
                      convolutional: half
                    ],
                    rateMatchingAttribute# 150 # crc_Size# crc16
                  }
                }
              }
            ]
            # ulTFCS#
            [
              normalTFCI_Signalling#
              [
                complete#
                {
                  ctfcSize#
                  [
                    ctfc2Bit#
                    [
                      {
                        ctfc2# 0 # powerOffsetInformation# OMIT
                      }
                      #
                      {
                        ctfc2# 1 # powerOffsetInformation# OMIT
                      }
                    ]
                  ]
                }
              ]
            ]
            # dlconnectedTrCHList# OMIT# dlTFCS# OMIT
          }
          # trCH_LogCHMapping#
          {
            ulconnectedTrCHList#
            [
              {
                trchid# 15 # trCH_LogCHMappingList#
                [
                  {
                    logicalChannel_Mapping#
                    [
                      ul_LogicalChannelMapping#
                      {
                        macHeaderManipulation# normalMacHeader# ul_TransportChannelType# rach# logicalChannelIdentity# 5 # logicalChannelType# cCCH
                      }
                    ]
                    # rB_Identity# 0 # cn_DomainIdentity# OMIT
                  }
                ]
              }
            ]
            # dlconnectedTrCHList# OMIT
          }
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          sS_rlc_Info:
          {
            sS_ul_RLC_Mode: OMIT,
            sS_dl_RLC_Mode:
            {
              dl_PayloadSize: 246,
              dl_RLCModeInfo:
              [
                ul_TM_RLC_Mode:
                {
                  transmissionRLC_Discard: OMIT,
                  segmentationIndication: GcFALSE
                }
              ]
            }
          },
          rB_LogCH_Mapping:
          {
            uLlogicalChannelIdentity: OMIT,
            dLlogicalChannelIdentity: 1,
            logicalChannelType: OMIT,
            cn_DomainIdentity: OMIT
          }
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -2
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          sS_rlc_Info:
          {
            sS_ul_RLC_Mode: OMIT,
            sS_dl_RLC_Mode:
            {
              dl_PayloadSize: 240,
              dl_RLCModeInfo:
              [
                ul_TM_RLC_Mode:
                {
                  transmissionRLC_Discard: OMIT,
                  segmentationIndication: GcFALSE
                }
              ]
            }
          },
          rB_LogCH_Mapping:
          {
            uLlogicalChannelIdentity: OMIT,
            dLlogicalChannelIdentity: 1,
            logicalChannelType: OMIT,
            cn_DomainIdentity: OMIT
          }
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: 0
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          sS_rlc_Info:
          {
            sS_ul_RLC_Mode: OMIT,
            sS_dl_RLC_Mode:
            {
              dl_PayloadSize: 152,
              dl_RLCModeInfo:
              [
                ul_UM_RLC_Mode:
                {
                  transmissionRLC_Discard:
                  [
                    timerBasedNoExplicit: dt100
                  ]
                }
              ]
            }
          },
          rB_LogCH_Mapping:
          {
            uLlogicalChannelIdentity: OMIT,
            dLlogicalChannelIdentity: 5,
            logicalChannelType: OMIT,
            cn_DomainIdentity: OMIT
          }
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: 0
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          sS_rlc_Info:
          {
            sS_ul_RLC_Mode:
            [
              dl_TM_RLC_Mode:
              {
                segmentationIndication: GcFALSE
              }
            ],
            sS_dl_RLC_Mode:
            {
              dl_PayloadSize: 166,
              dl_RLCModeInfo:
              [
                ul_TM_RLC_Mode:
                {
                  transmissionRLC_Discard: OMIT,
                  segmentationIndication: GcFALSE
                }
              ]
            }
          },
          rB_LogCH_Mapping:
          {
            uLlogicalChannelIdentity: 5,
            dLlogicalChannelIdentity: OMIT,
            logicalChannelType: OMIT,
            cn_DomainIdentity: OMIT
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 27,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              noSegment: NULL
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 11,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              completeSIB_List:
              [
                {
                  sib_Type: systemInformationBlockType1,
                  sib_Data_variable: '1100010000000000000001011000100000101000000010100001000000000000000001000000000000000000000011000111010000'B
                },

                {
                  sib_Type: systemInformationBlockType2,
                  sib_Data_variable: '00000000000000000010'B
                }
              ]
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 11,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              completeSIB_List:
              [
                {
                  sib_Type: systemInformationBlockType1,
                  sib_Data_variable: '1100010000000000000001011000100000101000000010100001000000000000000001000000000000000000000011000111010000'B
                },

                {
                  sib_Type: systemInformationBlockType2,
                  sib_Data_variable: '00000000000000000010'B
                }
              ]
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 10,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              completeSIB_List:
              [
                {
                  sib_Type: systemInformationBlockType7,
                  sib_Data_variable: '100000101000000010000001'B
                },

                {
                  sib_Type: systemInformationBlockType3,
                  sib_Data_variable: '0100000000000000000000000000110010110111000110000000000000010000000000100100001000000100011111111111111111111111'B
                }
              ]
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 26,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              completeSIB_List:
              [
                {
                  sib_Type: systemInformationBlockType7,
                  sib_Data_variable: '100000101000000010000001'B
                },

                {
                  sib_Type: systemInformationBlockType4,
                  sib_Data_variable: '00000000000000000000000000011001011011100011000000000000001000000000010010000000000010001110111'B
                }
              ]
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 23,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              noSegment: NULL
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 19,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              firstSegment:
              {
                sib_Type: systemInformationBlockType5,
                seg_Count: 3,
                sib_Data_fixed: '000101010100010000111110000000001111111101000011111111111111110111010010000100001111000000101001000011000000101010100101010110000000000000001100110001011011010101111110001010111010000011111110100000111111101000001111111010'B
              }
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 21,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              subsequentSegment:
              {
                sib_Type: systemInformationBlockType5,
                segmentIndex: 1,
                sib_Data_fixed: '000011111111010000000000000000001101011000110100010000111111010011100101000001100001000011001010000000110000001110000001000000010110000010000000111000000000100010000110010000101001100100001010000000000011000000010001000101'B
              }
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 22,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              lastSegmentShort:
              {
                sib_Type: systemInformationBlockType5,
                segmentIndex: 2,
                sib_Data_variable: '1100101011010110100000000000011110001000011000000001011011011011011000100000000001000011000010001001010000001011011010000000010000'B
              }
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 3,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              completeSIB_List:
              [
                {
                  sib_Type: systemInformationBlockType6,
                  sib_Data_variable: '0000001010010001'B
                }
              ]
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 5,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              noSegment: NULL
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 6,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              noSegment: NULL
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 7,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              noSegment: NULL
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 2,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              completeSIB_List:
              [
                {
                  sib_Type: systemInformationBlockType7,
                  sib_Data_variable: '100000101000000010000001'B
                }
              ]
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 10,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              completeSIB_List:
              [
                {
                  sib_Type: systemInformationBlockType7,
                  sib_Data_variable: '100000101000000010000001'B
                },

                {
                  sib_Type: systemInformationBlockType3,
                  sib_Data_variable: '0100000000000000000000000000110010110111000110000000000000010000000000100100001000000100011111111111111111111111'B
                }
              ]
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 18,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              completeSIB_List:
              [
                {
                  sib_Type: systemInformationBlockType7,
                  sib_Data_variable: '100000101000000010000001'B
                },

                {
                  sib_Type: systemInformationBlockType18,
                  sib_Data_variable: '100010000001000000000001000000001'B
                }
              ]
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 26,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              completeSIB_List:
              [
                {
                  sib_Type: systemInformationBlockType7,
                  sib_Data_variable: '100000101000000010000001'B
                },

                {
                  sib_Type: systemInformationBlockType4,
                  sib_Data_variable: '00000000000000000000000000011001011011100011000000000000001000000000010010000000000010001110111'B
                }
              ]
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 31,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              noSegment: NULL
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 29,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              firstSegment:
              {
                sib_Type: systemInformationBlockType11,
                seg_Count: 2,
                sib_Data_fixed: '001000001101100100001010001100001001111101000100100000010100101100101001010000101010111101000010001000100011001001010101000000010010100001010010101000011000010010100010000010100001000011000010010100100110101010000110000100'B
              }
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 30,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              lastSegmentShort:
              {
                sib_Type: systemInformationBlockType11,
                segmentIndex: 1,
                sib_Data_variable: '10101001001100000001010011100110000001000110010000100000100001001001011000100001000001001100100000100011000001011001000000100011100001011100001000'B
              }
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 13,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              completeSIB_List:
              [
                {
                  sib_Type: systemInformationBlockType12,
                  sib_Data_variable: '000000000'B
                }
              ]
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 14,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              noSegment: NULL
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 15,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              noSegment: NULL
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 18,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              completeSIB_List:
              [
                {
                  sib_Type: systemInformationBlockType7,
                  sib_Data_variable: '100000101000000010000001'B
                },

                {
                  sib_Type: systemInformationBlockType18,
                  sib_Data_variable: '100010000001000000000001000000001'B
                }
              ]
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 4,
        sg_POS: 1,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              completeSIB_List:
              [
                {
                  sib_Type: schedulingBlock1,
                  sib_Data_variable: '00010000101110001000001100110000010010010101111000101001110100000000010111100010001101110011100010010010'B
                }
              ]
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 3,
        sg_POS: 0,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              completeSIB_List:
              [
                {
                  sib_Type: masterInformationBlock,
                  sib_Data_variable: '0011000000000000100000000010010110101110000100010000000000100000100010110000111000100010110001011000100010100001111000100110100010011110010010010011000100010000'B
                }
              ]
            ]
          }
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 1
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 2
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 3
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 4
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CMAC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        physicalChannelIdentity: 26
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CMAC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        physicalChannelIdentity: 20
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CPHY_TrCH_Release_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        physicalChannelIdentity: 26
      ],
      trchConfigType:
      [
        dch: normal
      ]
    }

TTCN PDU: CPHY_TrCH_Release_CNF

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        physicalChannelIdentity: 26
      ]
    }

TTCN PDU: CPHY_TrCH_Release_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        physicalChannelIdentity: 20
      ],
      trchConfigType:
      [
        dch: normal
      ]
    }

TTCN PDU: CPHY_TrCH_Release_CNF

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        physicalChannelIdentity: 20
      ]
    }

TTCN PDU: CPHY_RL_Setup_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        physicalChannelIdentity: 26
      ],
      ratType: fdd,
      setupMessage:
      {
        physicalChannelInfo:
        [
          dPCHInfo:
          {
            ul_DPCHInfo: OMIT,
            dl_DPCHInfo:
            {
              dl_CommonInformation:
              {
                dl_DPCH_InfoCommon:
                {
                  cfnHandling:
                  [
                    initialise:
                    {
                      cfntargetsfnframeoffset: OMIT
                    }
                  ],
                  modeSpecificInfo:
                  [
                    fdd:
                    {
                      dl_DPCH_PowerControlInfo:
                      {
                        modeSpecificInfo:
                        [
                          fdd:
                          {
                            dpc_Mode: singleTPC
                          }
                        ]
                      },
                      powerOffsetPilot_pdpdch: 0,
                      dl_rate_matching_restriction: OMIT,
                      spreadingFactorAndPilot:
                      [
                        sfd128: pb4
                      ],
                      positionFixedOrFlexible: fixed,
                      tfci_Existence: GcFALSE
                    }
                  ]
                },
                modeSpecificInfo:
                [
                  fdd:
                  {
                    defaultDPCH_OffsetValue: 0,
                    dpch_CompressedModeInfo: OMIT,
                    tx_DiversityMode: noDiversity,
                    ssdt_Information: OMIT
                  }
                ]
              },
              dl_DPCH_InfoPerRL:
              [
                fdd:
                {
                  pCPICH_UsageForChannelEst: mayBeUsed,
                  dpch_FrameOffset: 0,
                  secondaryCPICH_Info: OMIT,
                  dl_ChannelisationCodeList:
                  [
                    {
                      secondaryScramblingCode: 1,
                      sf_AndCodeNumber:
                      [
                        sf128: 0
                      ],
                      scramblingCodeChange: OMIT
                    }
                  ],
                  tpc_CombinationIndex: 0,
                  ssdt_CellIdentity: OMIT,
                  closedLoopTimingAdjMode: OMIT
                }
              ],
              powerOffsetOfTFCI_PO1: 0,
              powerOffsetOfTPC_PO2: 0,
              powerOffsetOfPILOT_PO3: 0,
              dl_TxPower: -5,
              dl_TxPowerMax: 15,
              dl_TxPowerMin: -35
            }
          }
        ]
      }
    }

TTCN PDU: CPHY_TrCH_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        physicalChannelIdentity: 26
      ],
      ratType: fdd,
      trchConfigType:
      [
        dch: normal
      ],
      configMessage:
      {
        activationTime:
        [
          activateNow: NULL
        ],
        ulconnectedTrCHList: OMIT,
        ulTFCS: OMIT,
        dlconnectedTrCHList:
        [
          {
            trchid: 10,
            dl_TransportChannelType: dch,
            transportChannelInfo:
            {
              tti:
              [
                tti10:
                [
                  {
                    tb_Size: 148,
                    numberOfTbSizeList:
                    [
                      [
                        zero: NULL
                      ],

                      [
                        one: NULL
                      ]
                    ],
                    logicalChannelList:
                    [
                      allSizes: NULL
                    ]
                  }
                ]
              ],
              semistaticTF_Information:
              {
                channelCodingType:
                [
                  convolutional: third
                ],
                rateMatchingAttribute# 192 # crc_Size# crc16
              }
            }
          }
        ]
        # dlTFCS#
        [
          normalTFCI_Signalling#
          [
            complete#
            {
              ctfcSize#
              [
                ctfc2Bit#
                [
                  {
                    ctfc2# 0 # powerOffsetInformation#
                    {
                      gainFactorInformation#
                      [
                        computedGainFactors# 0
                      ]
                      # powerOffsetPp_m# OMIT
                    }
                  }
                  #
                  {
                    ctfc2# 1 # powerOffsetInformation#
                    {
                      gainFactorInformation#
                      [
                        signalledGainFactors#
                        {
                          modeSpecificInfo#
                          [
                            fdd#
                            {
                              gainFactorBetaC# 11
                            }
                          ]
                          # gainFactorBetaD# 15 # referenceTFC_ID# 0
                        }
                      ]
                      # powerOffsetPp_m# OMIT
                    }
                  }
                ]
              ]
            }
          ]
        ]
      }
    }

TTCN PDU: CPHY_TrCH_Config_CNF

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        physicalChannelIdentity: 26
      ]
    }

TTCN PDU: CMAC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        physicalChannelIdentity: 26
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          activationTime:
          [
            activateNow: NULL
          ],
          uE_Info:
          {
            u_RNTI: OMIT,
            c_RNTI: OMIT
          },
          trCHInfo:
          {
            ulconnectedTrCHList: OMIT,
            ulTFCS: OMIT,
            dlconnectedTrCHList:
            [
              {
                trchid: 10,
                transportChannelInfo:
                {
                  tti:
                  [
                    tti10:
                    [
                      {
                        tb_Size: 148,
                        numberOfTbSizeList:
                        [
                          [
                            zero: NULL
                          ],

                          [
                            one: NULL
                          ]
                        ],
                        logicalChannelList:
                        [
                          allSizes: NULL
                        ]
                      }
                    ]
                  ],
                  semistaticTF_Information:
                  {
                    channelCodingType:
                    [
                      convolutional: third
                    ],
                    rateMatchingAttribute# 192 # crc_Size# crc16
                  }
                }
              }
            ]
            # dlTFCS#
            [
              normalTFCI_Signalling#
              [
                complete#
                {
                  ctfcSize#
                  [
                    ctfc2Bit#
                    [
                      {
                        ctfc2# 0 # powerOffsetInformation#
                        {
                          gainFactorInformation#
                          [
                            computedGainFactors# 0
                          ]
                          # powerOffsetPp_m# OMIT
                        }
                      }
                      #
                      {
                        ctfc2# 1 # powerOffsetInformation#
                        {
                          gainFactorInformation#
                          [
                            signalledGainFactors#
                            {
                              modeSpecificInfo#
                              [
                                fdd#
                                {
                                  gainFactorBetaC# 11
                                }
                              ]
                              # gainFactorBetaD# 15 # referenceTFC_ID# 0
                            }
                          ]
                          # powerOffsetPp_m# OMIT
                        }
                      }
                    ]
                  ]
                }
              ]
            ]
          }
          # trCH_LogCHMapping#
          {
            ulconnectedTrCHList# OMIT# dlconnectedTrCHList#
            [
              {
                trchid# 10 # trCH_LogCHMappingList#
                [
                  {
                    logicalChannel_Mapping#
                    [
                      dl_LogicalChannelMapping#
                      {
                        macHeaderManipulation# normalMacHeader# dl_TransportChannelType# dch# logicalChannelIdentity# 1 # logicalChannelType# dCCH# rlc_SizeList#
                        [
                          configured# NULL
                        ]
                        # mac_LogicalChannelPriority# 1
                      }
                    ]
                    # rB_Identity# 1 # cn_DomainIdentity# OMIT
                  }
                  #
                  {
                    logicalChannel_Mapping#
                    [
                      dl_LogicalChannelMapping#
                      {
                        macHeaderManipulation# normalMacHeader# dl_TransportChannelType# dch# logicalChannelIdentity# 2 # logicalChannelType# dCCH# rlc_SizeList#
                        [
                          configured# NULL
                        ]
                        # mac_LogicalChannelPriority# 2
                      }
                    ]
                    # rB_Identity# 2 # cn_DomainIdentity# OMIT
                  }
                  #
                  {
                    logicalChannel_Mapping#
                    [
                      dl_LogicalChannelMapping#
                      {
                        macHeaderManipulation# normalMacHeader# dl_TransportChannelType# dch# logicalChannelIdentity# 3 # logicalChannelType# dCCH# rlc_SizeList#
                        [
                          configured# NULL
                        ]
                        # mac_LogicalChannelPriority# 3
                      }
                    ]
                    # rB_Identity# 3 # cn_DomainIdentity# OMIT
                  }
                  #
                  {
                    logicalChannel_Mapping#
                    [
                      dl_LogicalChannelMapping#
                      {
                        macHeaderManipulation# normalMacHeader# dl_TransportChannelType# dch# logicalChannelIdentity# 4 # logicalChannelType# dCCH# rlc_SizeList#
                        [
                          configured# NULL
                        ]
                        # mac_LogicalChannelPriority# 4
                      }
                    ]
                    # rB_Identity# 4 # cn_DomainIdentity# OMIT
                  }
                ]
              }
            ]
          }
        }
      ]
    }

TTCN PDU: CPHY_RL_Setup_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        physicalChannelIdentity: 20
      ],
      ratType: fdd,
      setupMessage:
      {
        physicalChannelInfo:
        [
          dPCHInfo:
          {
            ul_DPCHInfo:
            {
              ul_DPCH_PowerControlInfo:
              [
                fdd:
                {
                  dpcch_PowerOffset: -40,
                  pc_Preamble: 1,
                  sRB_delay: 7,
                  powerControlAlgorithm:
                  [
                    algorithm1: 0
                  ]
                }
              ],
              modeSpecificInfo:
              [
                fdd:
                {
                  scramblingCodeType: longSC,
                  scramblingCode: 3000,
                  numberOfDPDCH: OMIT,
                  spreadingFactor: sf64,
                  tfci_Existence: GcTRUE,
                  numberOfFBI_Bits: OMIT,
                  puncturingLimit: pl1
                }
              ]
            },
            dl_DPCHInfo: OMIT
          }
        ]
      }
    }

TTCN PDU: CPHY_TrCH_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        physicalChannelIdentity: 20
      ],
      ratType: fdd,
      trchConfigType:
      [
        dch: normal
      ],
      configMessage:
      {
        activationTime:
        [
          activateNow: NULL
        ],
        ulconnectedTrCHList:
        [
          {
            trchid: 5,
            ul_TransportChannelType: dch,
            transportChannelInfo:
            {
              tti:
              [
                tti10:
                [
                  {
                    tb_Size: 148,
                    numberOfTbSizeList:
                    [
                      [
                        zero: NULL
                      ],

                      [
                        one: NULL
                      ]
                    ],
                    logicalChannelList:
                    [
                      allSizes: NULL
                    ]
                  }
                ]
              ],
              semistaticTF_Information:
              {
                channelCodingType:
                [
                  convolutional: third
                ],
                rateMatchingAttribute# 192 # crc_Size# crc16
              }
            }
          }
        ]
        # ulTFCS#
        [
          normalTFCI_Signalling#
          [
            complete#
            {
              ctfcSize#
              [
                ctfc2Bit#
                [
                  {
                    ctfc2# 0 # powerOffsetInformation# OMIT
                  }
                  #
                  {
                    ctfc2# 1 # powerOffsetInformation# OMIT
                  }
                ]
              ]
            }
          ]
        ]
        # dlconnectedTrCHList# OMIT# dlTFCS# OMIT
      }
    }

TTCN PDU: CPHY_TrCH_Config_CNF

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        physicalChannelIdentity: 20
      ]
    }

TTCN PDU: CMAC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        physicalChannelIdentity: 20
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          activationTime:
          [
            activateNow: NULL
          ],
          uE_Info:
          {
            u_RNTI: OMIT,
            c_RNTI: OMIT
          },
          trCHInfo:
          {
            ulconnectedTrCHList:
            [
              {
                trchid: 5,
                transportChannelInfo:
                {
                  tti:
                  [
                    tti10:
                    [
                      {
                        tb_Size: 148,
                        numberOfTbSizeList:
                        [
                          [
                            zero: NULL
                          ],

                          [
                            one: NULL
                          ]
                        ],
                        logicalChannelList:
                        [
                          allSizes: NULL
                        ]
                      }
                    ]
                  ],
                  semistaticTF_Information:
                  {
                    channelCodingType:
                    [
                      convolutional: third
                    ],
                    rateMatchingAttribute# 192 # crc_Size# crc16
                  }
                }
              }
            ]
            # ulTFCS#
            [
              normalTFCI_Signalling#
              [
                complete#
                {
                  ctfcSize#
                  [
                    ctfc2Bit#
                    [
                      {
                        ctfc2# 0 # powerOffsetInformation# OMIT
                      }
                      #
                      {
                        ctfc2# 1 # powerOffsetInformation# OMIT
                      }
                    ]
                  ]
                }
              ]
            ]
            # dlconnectedTrCHList# OMIT# dlTFCS# OMIT
          }
          # trCH_LogCHMapping#
          {
            ulconnectedTrCHList#
            [
              {
                trchid# 5 # trCH_LogCHMappingList#
                [
                  {
                    logicalChannel_Mapping#
                    [
                      ul_LogicalChannelMapping#
                      {
                        macHeaderManipulation# normalMacHeader# ul_TransportChannelType# dch# logicalChannelIdentity# 1 # logicalChannelType# dCCH
                      }
                    ]
                    # rB_Identity# 1 # cn_DomainIdentity# OMIT
                  }
                  #
                  {
                    logicalChannel_Mapping#
                    [
                      ul_LogicalChannelMapping#
                      {
                        macHeaderManipulation# normalMacHeader# ul_TransportChannelType# dch# logicalChannelIdentity# 2 # logicalChannelType# dCCH
                      }
                    ]
                    # rB_Identity# 2 # cn_DomainIdentity# OMIT
                  }
                  #
                  {
                    logicalChannel_Mapping#
                    [
                      ul_LogicalChannelMapping#
                      {
                        macHeaderManipulation# normalMacHeader# ul_TransportChannelType# dch# logicalChannelIdentity# 3 # logicalChannelType# dCCH
                      }
                    ]
                    # rB_Identity# 3 # cn_DomainIdentity# OMIT
                  }
                  #
                  {
                    logicalChannel_Mapping#
                    [
                      ul_LogicalChannelMapping#
                      {
                        macHeaderManipulation# normalMacHeader# ul_TransportChannelType# dch# logicalChannelIdentity# 4 # logicalChannelType# dCCH
                      }
                    ]
                    # rB_Identity# 4 # cn_DomainIdentity# OMIT
                  }
                ]
              }
            ]
            # dlconnectedTrCHList# OMIT
          }
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 1
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          sS_rlc_Info:
          {
            sS_ul_RLC_Mode:
            [
              dl_UM_RLC_Mode: NULL
            ],
            sS_dl_RLC_Mode:
            {
              dl_PayloadSize: 136,
              dl_RLCModeInfo:
              [
                ul_UM_RLC_Mode:
                {
                  transmissionRLC_Discard:
                  [
                    timerBasedNoExplicit: dt100
                  ]
                }
              ]
            }
          },
          rB_LogCH_Mapping:
          {
            uLlogicalChannelIdentity: 1,
            dLlogicalChannelIdentity: 1,
            logicalChannelType: OMIT,
            cn_DomainIdentity: OMIT
          }
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 2
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          sS_rlc_Info:
          {
            sS_ul_RLC_Mode:
            [
              dl_AM_RLC_Mode:
              {
                inSequenceDelivery: GcTRUE,
                receivingWindowSize: rw32,
                dl_RLC_StatusInfo:
                {
                  timerStatusProhibit: tsp200,
                  timerEPC: OMIT,
                  missingPDU_Indicator: GcTRUE,
                  timerStatusPeriodic: OMIT
                }
              }
            ],
            sS_dl_RLC_Mode:
            {
              dl_PayloadSize: 128,
              dl_RLCModeInfo:
              [
                ul_AM_RLC_Mode:
                {
                  transmissionRLC_Discard:
                  [
                    noDiscard: dat15
                  ],
                  transmissionWindowSize: tw32,
                  timerRST: tr500,
                  max_RST: rst1,
                  pollingInfo:
                  {
                    timerPollProhibit: tpp200,
                    timerPoll: tp200,
                    poll_PDU: OMIT,
                    poll_SDU: sdu1,
                    lastTransmissionPDU_Poll: GcTRUE,
                    lastRetransmissionPDU_Poll: GcTRUE,
                    pollWindow: pw99,
                    timerPollPeriodic: OMIT
                  }
                }
              ]
            }
          },
          rB_LogCH_Mapping:
          {
            uLlogicalChannelIdentity: 2,
            dLlogicalChannelIdentity: 2,
            logicalChannelType: OMIT,
            cn_DomainIdentity: OMIT
          }
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 3
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          sS_rlc_Info:
          {
            sS_ul_RLC_Mode:
            [
              dl_AM_RLC_Mode:
              {
                inSequenceDelivery: GcTRUE,
                receivingWindowSize: rw32,
                dl_RLC_StatusInfo:
                {
                  timerStatusProhibit: tsp200,
                  timerEPC: OMIT,
                  missingPDU_Indicator: GcTRUE,
                  timerStatusPeriodic: OMIT
                }
              }
            ],
            sS_dl_RLC_Mode:
            {
              dl_PayloadSize: 128,
              dl_RLCModeInfo:
              [
                ul_AM_RLC_Mode:
                {
                  transmissionRLC_Discard:
                  [
                    noDiscard: dat15
                  ],
                  transmissionWindowSize: tw32,
                  timerRST: tr500,
                  max_RST: rst1,
                  pollingInfo:
                  {
                    timerPollProhibit: tpp200,
                    timerPoll: tp200,
                    poll_PDU: OMIT,
                    poll_SDU: sdu1,
                    lastTransmissionPDU_Poll: GcTRUE,
                    lastRetransmissionPDU_Poll: GcTRUE,
                    pollWindow: pw99,
                    timerPollPeriodic: OMIT
                  }
                }
              ]
            }
          },
          rB_LogCH_Mapping:
          {
            uLlogicalChannelIdentity: 3,
            dLlogicalChannelIdentity: 3,
            logicalChannelType: OMIT,
            cn_DomainIdentity: OMIT
          }
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 4
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          sS_rlc_Info:
          {
            sS_ul_RLC_Mode:
            [
              dl_AM_RLC_Mode:
              {
                inSequenceDelivery: GcTRUE,
                receivingWindowSize: rw32,
                dl_RLC_StatusInfo:
                {
                  timerStatusProhibit: tsp200,
                  timerEPC: OMIT,
                  missingPDU_Indicator: GcTRUE,
                  timerStatusPeriodic: OMIT
                }
              }
            ],
            sS_dl_RLC_Mode:
            {
              dl_PayloadSize: 128,
              dl_RLCModeInfo:
              [
                ul_AM_RLC_Mode:
                {
                  transmissionRLC_Discard:
                  [
                    noDiscard: dat15
                  ],
                  transmissionWindowSize: tw32,
                  timerRST: tr500,
                  max_RST: rst1,
                  pollingInfo:
                  {
                    timerPollProhibit: tpp200,
                    timerPoll: tp200,
                    poll_PDU: OMIT,
                    poll_SDU: sdu1,
                    lastTransmissionPDU_Poll: GcTRUE,
                    lastRetransmissionPDU_Poll: GcTRUE,
                    pollWindow: pw99,
                    timerPollPeriodic: OMIT
                  }
                }
              ]
            }
          },
          rB_LogCH_Mapping:
          {
            uLlogicalChannelIdentity: 4,
            dLlogicalChannelIdentity: 4,
            logicalChannelType: OMIT,
            cn_DomainIdentity: OMIT
          }
        }
      ]
    }

TTCN PDU: RLC_TR_DATA_IND

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: 0
      ],
      tM_message:
      [
        uL_CCCH_Message: PDU:
        {
          integrityCheckInfo: OMIT,
          message:
          [
            rrcConnectionRequest:
            {
              initialUE_Identity:
              [
                imsi:
                [
                  0,
                  0,
                  1,
                  0,
                  1,
                  0,
                  0,
                  0,
                  0,
                  0,
                  0,
                  0,
                  3,
                  3,
                  3
                ]
              ],
              establishmentCause: registration,
              protocolErrorIndicator: noError,
              measuredResultsOnRACH: OMIT,
              v3d0NonCriticalExtensions: OMIT
            }
          ]
        }
      ]
    }

TTCN PDU: RLC_UM_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: 0
      ],
      uM_message:
      [
        dL_CCCH_Message: PDU:
        {
          integrityCheckInfo: OMIT,
          message:
          [
            rrcConnectionSetup:
            [
              r3:
              {
                rrcConnectionSetup_r3:
                {
                  initialUE_Identity:
                  [
                    imsi:
                    [
                      0,
                      0,
                      1,
                      0,
                      1,
                      0,
                      0,
                      0,
                      0,
                      0,
                      0,
                      0,
                      3,
                      3,
                      3
                    ]
                  ],
                  rrc_TransactionIdentifier: 0,
                  activationTime: OMIT,
                  new_U_RNTI:
                  {
                    srnc_Identity: '000000000001'B,
                    s_RNTI: '00000000000000000001'B
                  },
                  new_c_RNTI: OMIT,
                  rrc_StateIndicator: cell_DCH,
                  utran_DRX_CycleLengthCoeff: 9,
                  capabilityUpdateRequirement:
                  {
                    ue_RadioCapabilityFDDUpdateRequirement: GcTRUE,
                    ue_RadioCapabilityTDDUpdateRequirement: GcFALSE,
                    systemSpecificCapUpdateReqList:
                    [
                      gsm
                    ]
                  },
                  srb_InformationSetupList:
                  [
                    {
                      rb_Identity: OMIT,
                      rlc_InfoChoice:
                      [
                        rlc_Info:
                        {
                          ul_RLC_Mode:
                          [
                            ul_UM_RLC_Mode:
                            {
                              transmissionRLC_Discard: OMIT
                            }
                          ],
                          dl_RLC_Mode:
                          [
                            dl_UM_RLC_Mode: NULL
                          ]
                        }
                      ],
                      rb_MappingInfo:
                      [
                        {
                          ul_LogicalChannelMappings:
                          [
                            oneLogicalChannel:
                            {
                              ul_TransportChannelType:
                              [
                                dch: 5
                              ],
                              logicalChannelIdentity: 1,
                              rlc_SizeList:
                              [
                                configured: NULL
                              ],
                              mac_LogicalChannelPriority: 1
                            }
                          ],
                          dl_LogicalChannelMappingList:
                          [
                            {
                              dl_TransportChannelType:
                              [
                                dch: 10
                              ],
                              logicalChannelIdentity: 1
                            }
                          ]
                        },

                        {
                          ul_LogicalChannelMappings:
                          [
                            oneLogicalChannel:
                            {
                              ul_TransportChannelType:
                              [
                                rach: NULL
                              ],
                              logicalChannelIdentity: 1,
                              rlc_SizeList:
                              [
                                explicitList:
                                [
                                  {
                                    rlc_SizeIndex: 1
                                  }
                                ]
                              ],
                              mac_LogicalChannelPriority: 1
                            }
                          ],
                          dl_LogicalChannelMappingList:
                          [
                            {
                              dl_TransportChannelType:
                              [
                                fach: NULL
                              ],
                              logicalChannelIdentity: 1
                            }
                          ]
                        }
                      ]
                    },

                    {
                      rb_Identity: OMIT,
                      rlc_InfoChoice:
                      [
                        rlc_Info:
                        {
                          ul_RLC_Mode:
                          [
                            ul_AM_RLC_Mode:
                            {
                              transmissionRLC_Discard:
                              [
                                noDiscard: dat15
                              ],
                              transmissionWindowSize: tw32,
                              timerRST: tr500,
                              max_RST: rst1,
                              pollingInfo:
                              {
                                timerPollProhibit: tpp200,
                                timerPoll: tp200,
                                poll_PDU: OMIT,
                                poll_SDU: sdu1,
                                lastTransmissionPDU_Poll: GcTRUE,
                                lastRetransmissionPDU_Poll: GcTRUE,
                                pollWindow: pw99,
                                timerPollPeriodic: OMIT
                              }
                            }
                          ],
                          dl_RLC_Mode:
                          [
                            dl_AM_RLC_Mode:
                            {
                              inSequenceDelivery: GcTRUE,
                              receivingWindowSize: rw32,
                              dl_RLC_StatusInfo:
                              {
                                timerStatusProhibit: tsp200,
                                timerEPC: OMIT,
                                missingPDU_Indicator: GcTRUE,
                                timerStatusPeriodic: OMIT
                              }
                            }
                          ]
                        }
                      ],
                      rb_MappingInfo:
                      [
                        {
                          ul_LogicalChannelMappings:
                          [
                            oneLogicalChannel:
                            {
                              ul_TransportChannelType:
                              [
                                dch: 5
                              ],
                              logicalChannelIdentity: 2,
                              rlc_SizeList:
                              [
                                configured: NULL
                              ],
                              mac_LogicalChannelPriority: 2
                            }
                          ],
                          dl_LogicalChannelMappingList:
                          [
                            {
                              dl_TransportChannelType:
                              [
                                dch: 10
                              ],
                              logicalChannelIdentity: 2
                            }
                          ]
                        },

                        {
                          ul_LogicalChannelMappings:
                          [
                            oneLogicalChannel:
                            {
                              ul_TransportChannelType:
                              [
                                rach: NULL
                              ],
                              logicalChannelIdentity: 2,
                              rlc_SizeList:
                              [
                                explicitList:
                                [
                                  {
                                    rlc_SizeIndex: 1
                                  }
                                ]
                              ],
                              mac_LogicalChannelPriority: 2
                            }
                          ],
                          dl_LogicalChannelMappingList:
                          [
                            {
                              dl_TransportChannelType:
                              [
                                fach: NULL
                              ],
                              logicalChannelIdentity: 2
                            }
                          ]
                        }
                      ]
                    },

                    {
                      rb_Identity: OMIT,
                      rlc_InfoChoice:
                      [
                        rlc_Info:
                        {
                          ul_RLC_Mode:
                          [
                            ul_AM_RLC_Mode:
                            {
                              transmissionRLC_Discard:
                              [
                                noDiscard: dat15
                              ],
                              transmissionWindowSize: tw32,
                              timerRST: tr500,
                              max_RST: rst1,
                              pollingInfo:
                              {
                                timerPollProhibit: tpp200,
                                timerPoll: tp200,
                                poll_PDU: OMIT,
                                poll_SDU: sdu1,
                                lastTransmissionPDU_Poll: GcTRUE,
                                lastRetransmissionPDU_Poll: GcTRUE,
                                pollWindow: pw99,
                                timerPollPeriodic: OMIT
                              }
                            }
                          ],
                          dl_RLC_Mode:
                          [
                            dl_AM_RLC_Mode:
                            {
                              inSequenceDelivery: GcTRUE,
                              receivingWindowSize: rw32,
                              dl_RLC_StatusInfo:
                              {
                                timerStatusProhibit: tsp200,
                                timerEPC: OMIT,
                                missingPDU_Indicator: GcTRUE,
                                timerStatusPeriodic: OMIT
                              }
                            }
                          ]
                        }
                      ],
                      rb_MappingInfo:
                      [
                        {
                          ul_LogicalChannelMappings:
                          [
                            oneLogicalChannel:
                            {
                              ul_TransportChannelType:
                              [
                                dch: 5
                              ],
                              logicalChannelIdentity: 3,
                              rlc_SizeList:
                              [
                                configured: NULL
                              ],
                              mac_LogicalChannelPriority: 3
                            }
                          ],
                          dl_LogicalChannelMappingList:
                          [
                            {
                              dl_TransportChannelType:
                              [
                                dch: 10
                              ],
                              logicalChannelIdentity: 3
                            }
                          ]
                        },

                        {
                          ul_LogicalChannelMappings:
                          [
                            oneLogicalChannel:
                            {
                              ul_TransportChannelType:
                              [
                                rach: NULL
                              ],
                              logicalChannelIdentity: 3,
                              rlc_SizeList:
                              [
                                explicitList:
                                [
                                  {
                                    rlc_SizeIndex: 1
                                  }
                                ]
                              ],
                              mac_LogicalChannelPriority: 3
                            }
                          ],
                          dl_LogicalChannelMappingList:
                          [
                            {
                              dl_TransportChannelType:
                              [
                                fach: NULL
                              ],
                              logicalChannelIdentity: 3
                            }
                          ]
                        }
                      ]
                    },

                    {
                      rb_Identity: OMIT,
                      rlc_InfoChoice:
                      [
                        rlc_Info:
                        {
                          ul_RLC_Mode:
                          [
                            ul_AM_RLC_Mode:
                            {
                              transmissionRLC_Discard:
                              [
                                noDiscard: dat15
                              ],
                              transmissionWindowSize: tw32,
                              timerRST: tr500,
                              max_RST: rst1,
                              pollingInfo:
                              {
                                timerPollProhibit: tpp200,
                                timerPoll: tp200,
                                poll_PDU: OMIT,
                                poll_SDU: sdu1,
                                lastTransmissionPDU_Poll: GcTRUE,
                                lastRetransmissionPDU_Poll: GcTRUE,
                                pollWindow: pw99,
                                timerPollPeriodic: OMIT
                              }
                            }
                          ],
                          dl_RLC_Mode:
                          [
                            dl_AM_RLC_Mode:
                            {
                              inSequenceDelivery: GcTRUE,
                              receivingWindowSize: rw32,
                              dl_RLC_StatusInfo:
                              {
                                timerStatusProhibit: tsp200,
                                timerEPC: OMIT,
                                missingPDU_Indicator: GcTRUE,
                                timerStatusPeriodic: OMIT
                              }
                            }
                          ]
                        }
                      ],
                      rb_MappingInfo:
                      [
                        {
                          ul_LogicalChannelMappings:
                          [
                            oneLogicalChannel:
                            {
                              ul_TransportChannelType:
                              [
                                dch: 5
                              ],
                              logicalChannelIdentity: 4,
                              rlc_SizeList:
                              [
                                configured: NULL
                              ],
                              mac_LogicalChannelPriority: 4
                            }
                          ],
                          dl_LogicalChannelMappingList:
                          [
                            {
                              dl_TransportChannelType:
                              [
                                dch: 10
                              ],
                              logicalChannelIdentity: 4
                            }
                          ]
                        },

                        {
                          ul_LogicalChannelMappings:
                          [
                            oneLogicalChannel:
                            {
                              ul_TransportChannelType:
                              [
                                rach: NULL
                              ],
                              logicalChannelIdentity: 4,
                              rlc_SizeList:
                              [
                                explicitList:
                                [
                                  {
                                    rlc_SizeIndex: 1
                                  }
                                ]
                              ],
                              mac_LogicalChannelPriority: 4
                            }
                          ],
                          dl_LogicalChannelMappingList:
                          [
                            {
                              dl_TransportChannelType:
                              [
                                fach: NULL
                              ],
                              logicalChannelIdentity: 4
                            }
                          ]
                        }
                      ]
                    }
                  ],
                  ul_CommonTransChInfo:
                  {
                    tfc_Subset: OMIT,
                    prach_TFCS: OMIT,
                    modeSpecificInfo:
                    [
                      fdd:
                      {
                        ul_TFCS:
                        [
                          normalTFCI_Signalling:
                          [
                            complete:
                            {
                              ctfcSize:
                              [
                                ctfc2Bit:
                                [
                                  {
                                    ctfc2: 0,
                                    powerOffsetInformation:
                                    {
                                      gainFactorInformation:
                                      [
                                        computedGainFactors: 0
                                      ],
                                      powerOffsetPp_m: OMIT
                                    }
                                  },

                                  {
                                    ctfc2: 1,
                                    powerOffsetInformation:
                                    {
                                      gainFactorInformation:
                                      [
                                        signalledGainFactors:
                                        {
                                          modeSpecificInfo:
                                          [
                                            fdd:
                                            {
                                              gainFactorBetaC: 11
                                            }
                                          ],
                                          gainFactorBetaD: 15,
                                          referenceTFC_ID: 0
                                        }
                                      ],
                                      powerOffsetPp_m: OMIT
                                    }
                                  }
                                ]
                              ]
                            }
                          ]
                        ]
                      }
                    ]
                  },
                  ul_AddReconfTransChInfoList:
                  [
                    {
                      ul_TransportChannelType: dch,
                      transportChannelIdentity: 5,
                      transportFormatSet:
                      [
                        dedicatedTransChTFS:
                        {
                          tti:
                          [
                            tti10:
                            [
                              {
                                rlc_Size:
                                [
                                  bitMode:
                                  [
                                    sizeType2:
                                    {
                                      part1: 2,
                                      part2: OMIT
                                    }
                                  ]
                                ],
                                numberOfTbSizeList:
                                [
                                  [
                                    zero: NULL
                                  ],

                                  [
                                    one: NULL
                                  ]
                                ],
                                logicalChannelList:
                                [
                                  allSizes: NULL
                                ]
                              }
                            ]
                          ],
                          semistaticTF_Information:
                          {
                            channelCodingType:
                            [
                              convolutional: third
                            ],
                            rateMatchingAttribute# 192 # crc_Size# crc16
                          }
                        }
                      ]
                    }
                  ]
                  # dl_CommonTransChInfo#
                  {
                    sccpch_TFCS# OMIT# modeSpecificInfo#
                    [
                      fdd#
                      {
                        dl_Parameters#
                        [
                          sameAsUL# NULL
                        ]
                      }
                    ]
                  }
                  # dl_AddReconfTransChInfoList#
                  [
                    {
                      dl_TransportChannelType# dch# dl_transportChannelIdentity# 10 # tfs_SignallingMode#
                      [
                        sameAsULTrCH#
                        {
                          ul_TransportChannelType# dch# ul_TransportChannelIdentity# 5
                        }
                      ]
                      # dch_QualityTarget#
                      {
                        bler_QualityValue# #20
                      }
                      # dummy# OMIT
                    }
                  ]
                  # frequencyInfo# OMIT# maxAllowedUL_TX_Power# OMIT# ul_ChannelRequirement#
                  [
                    ul_DPCH_Info#
                    {
                      ul_DPCH_PowerControlInfo#
                      [
                        fdd#
                        {
                          dpcch_PowerOffset# #40 # pc_Preamble# 1 # sRB_delay# 7 # powerControlAlgorithm#
                          [
                            algorithm1# 0
                          ]
                        }
                      ]
                      # modeSpecificInfo#
                      [
                        fdd#
                        {
                          scramblingCodeType# longSC# scramblingCode# 3000 # numberOfDPDCH# OMIT# spreadingFactor# sf64# tfci_Existence# GcTRUE # numberOfFBI_Bits# OMIT# puncturingLimit# pl1
                        }
                      ]
                    }
                  ]
                  # dl_CommonInformation#
                  {
                    dl_DPCH_InfoCommon#
                    {
                      cfnHandling#
                      [
                        initialise#
                        {
                          cfntargetsfnframeoffset# OMIT
                        }
                      ]
                      # modeSpecificInfo#
                      [
                        fdd#
                        {
                          dl_DPCH_PowerControlInfo#
                          {
                            modeSpecificInfo#
                            [
                              fdd#
                              {
                                dpc_Mode# singleTPC
                              }
                            ]
                          }
                          # powerOffsetPilot_pdpdch# 0 # dl_rate_matching_restriction# OMIT# spreadingFactorAndPilot#
                          [
                            sfd128# pb4
                          ]
                          # positionFixedOrFlexible# fixed# tfci_Existence# GcFALSE
                        }
                      ]
                    }
                    # modeSpecificInfo#
                    [
                      fdd#
                      {
                        defaultDPCH_OffsetValue# 0 # dpch_CompressedModeInfo# OMIT# tx_DiversityMode# noDiversity# ssdt_Information# OMIT
                      }
                    ]
                  }
                  # dl_InformationPerRL_List#
                  [
                    {
                      modeSpecificInfo#
                      [
                        fdd#
                        {
                          primaryCPICH_Info#
                          {
                            primaryScramblingCode# 250
                          }
                          # pdsch_SHO_DCH_Info# OMIT# pdsch_CodeMapping# OMIT
                        }
                      ]
                      # dl_DPCH_InfoPerRL#
                      [
                        fdd#
                        {
                          pCPICH_UsageForChannelEst# mayBeUsed# dpch_FrameOffset# 0 # secondaryCPICH_Info# OMIT# dl_ChannelisationCodeList#
                          [
                            {
                              secondaryScramblingCode# 1 # sf_AndCodeNumber#
                              [
                                sf128# 0
                              ]
                              # scramblingCodeChange# noCodeChange
                            }
                          ]
                          # tpc_CombinationIndex# 0 # ssdt_CellIdentity# OMIT# closedLoopTimingAdjMode# OMIT
                        }
                      ]
                      # sccpch_InfoforFACH# OMIT
                    }
                  ]
                }
                # laterNonCriticalExtensions# OMIT
              }
            ]
          ]
        }
      ]
      # specialLI# GcTRUE
    }

TTCN PDU: RLC_AM_DATA_IND

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 2
      ],
      integrityResult:
      [
        integrityUsed: i_pass
      ],
      aM_message:
      [
        uL_DCCH_Message: PDU:
        {
          integrityCheckInfo: OMIT,
          message:
          [
            rrcConnectionSetupComplete:
            {
              rrc_TransactionIdentifier: 0,
              startList:
              [
                {
                  cn_DomainIdentity: ps_domain,
                  start_Value: '00000000000000000010'B
                },

                {
                  cn_DomainIdentity: cs_domain,
                  start_Value: '00000000000000000010'B
                }
              ],
              ue_RadioAccessCapability:
              {
                accessStratumReleaseIndicator: r99,
                pdcp_Capability:
                {
                  losslessSRNS_RelocationSupport: GcFALSE,
                  supportForRfc2507:
                  [
                    notSupported: NULL
                  ]
                },
                rlc_Capability:
                {
                  totalRLC_AM_BufferSize: kb50,
                  maximumRLC_WindowSize: mws2047,
                  maximumAM_EntityNumber: am6
                },
                transportChannelCapability:
                {
                  dl_TransChCapability:
                  {
                    maxNoBitsReceived: b8960,
                    maxConvCodeBitsReceived: b1280,
                    turboDecodingSupport:
                    [
                      supported: b8960
                    ],
                    maxSimultaneousTransChs: e8,
                    maxSimultaneousCCTrCH_Count: 1,
                    maxReceivedTransportBlocks: tb32,
                    maxNumberOfTFC: tfc128,
                    maxNumberOfTF: tf64
                  },
                  ul_TransChCapability:
                  {
                    maxNoBitsTransmitted: b3840,
                    maxConvCodeBitsTransmitted: b1280,
                    turboEncodingSupport:
                    [
                      supported: b3840
                    ],
                    maxSimultaneousTransChs: e8,
                    modeSpecificInfo:
                    [
                      fdd: NULL
                    ],
                    maxTransmittedBlocks: tb32,
                    maxNumberOfTFC: tfc64,
                    maxNumberOfTF: tf32
                  }
                },
                rf_Capability:
                {
                  fddRF_Capability:
                  {
                    ue_PowerClass: 4,
                    txRxFrequencySeparation: mhz190
                  },
                  tddRF_Capability: OMIT
                },
                physicalChannelCapability:
                {
                  fddPhysChCapability:
                  {
                    downlinkPhysChCapability:
                    {
                      maxNoDPCH_PDSCH_Codes: 1,
                      maxNoPhysChBitsReceived: b9600,
                      supportForSF_512: GcFALSE,
                      supportOfPDSCH: GcFALSE,
                      simultaneousSCCPCH_DPCH_Reception:
                      [
                        notSupported: NULL
                      ]
                    },
                    uplinkPhysChCapability:
                    {
                      maxNoDPDCH_BitsTransmitted: b4800,
                      supportOfPCPCH: GcFALSE
                    }
                  },
                  tddPhysChCapability: OMIT
                },
                ue_MultiModeRAT_Capability:
                {
                  multiRAT_CapabilityList:
                  {
                    supportOfGSM: GcFALSE,
                    supportOfMulticarrier: GcFALSE
                  },
                  multiModeCapability: fdd
                },
                securityCapability:
                {
                  cipheringAlgorithmCap: '0000000000000011'B,
                  integrityProtectionAlgorithmCap: '0000000000000010'B
                },
                ue_positioning_Capability:
                {
                  standaloneLocMethodsSupported: GcFALSE,
                  ue_BasedOTDOA_Supported: GcFALSE,
                  networkAssistedGPS_Supported: noNetworkAssistedGPS,
                  supportForUE_GPS_TimingOfCellFrames: GcFALSE,
                  supportForIPDL: GcFALSE
                },
                measurementCapability:
                {
                  downlinkCompressedMode:
                  {
                    fdd_Measurements: GcTRUE,
                    tdd_Measurements: OMIT,
                    gsm_Measurements:
                    {
                      gsm900: GcTRUE,
                      dcs1800: GcTRUE,
                      gsm1900: GcTRUE
                    },
                    multiCarrierMeasurements: GcFALSE
                  },
                  uplinkCompressedMode:
                  {
                    fdd_Measurements: GcTRUE,
                    tdd_Measurements: OMIT,
                    gsm_Measurements:
                    {
                      gsm900: GcTRUE,
                      dcs1800: GcTRUE,
                      gsm1900: GcTRUE
                    },
                    multiCarrierMeasurements: GcFALSE
                  }
                }
              },
              ue_RATSpecificCapability: OMIT,
              v370NonCriticalExtensions: OMIT
            }
          ]
        }
      ]
    }

TTCN PDU: RRC_DataInd

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      rB_Id: 3,
      ch: OMIT,
      sapId: OMIT,
      cN_Domain: 0,
      start: '00000000000000000010'B,
      msg: PDU:
      {
        skipIndicator: '0000'B,
        mMProtocolDiscriminator: '0101'B,
        msgType: '00001000'B,
        ciphKeySeqNum:
        {
          spare1: '0'B,
          keySeq: '111'B
        },
        locUpdType:
        {
          fOR: '0'B,
          spare1: '0'B,
          lUT: '00'B
        },
        locAreaId:
        {
          plmn: '00F110'O,
          lac: 'FFFE'O
        },
        mSClsmk1:
        {
          spare1: '0'B,
          revLvl: '10'B,
          eSIND: '0'B,
          a5_1: '1'B,
          rFPwrCap: '111'B
        },
        mobileId:
        {
          iel: '08'O,
          iDigit1: '0000'B,
          oddEvenInd: '1'B,
          typeOfId: '001'B,
          otherDigits: '10100000003033'O
        },
        mSClsmk2:
        {
          iei: '00110011'B,
          iel: '03'O,
          spare1_1: '0'B,
          revLvl: '10'B,
          eSIND: '0'B,
          a5_1: '1'B,
          rFPwrCap: '111'B,
          spare1_2: '0'B,
          pSCap: '0'B,
          sSSI: '01'B,
          sMCap: '1'B,
          vBS: '0'B,
          vGCS: '0'B,
          fC: '0'B,
          cM3: '1'B,
          spare1_3: '0'B,
          lCSVA: '1'B,
          uCS2: '0'B,
          soLSA: '0'B,
          cMSP: '0'B,
          a5_3: '0'B,
          a5_2: '0'B
        }
      }
    }

TTCN PDU: RRC_DataReq

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      rB_Id: 3,
      ch: OMIT,
      sapId: OMIT,
      cN_Domain: 0,
      msg: PDU:
      {
        skipIndicator: '0000'B,
        mMProtocolDiscriminator: '0101'B,
        msgType: '00010010'B,
        spare4: '0000'B,
        ciphKeySeqNum:
        {
          spare1: '0'B,
          keySeq: '001'B
        },
        rAND: '01010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101'B,
        aUTN:
        {
          iei: '00100000'B,
          iel: '10'O,
          aUTN: '01100110000100010000000000110011001000101101110100000000000000000101010101000100011101110110011000010001000000000011001100100010'B
        }
      }
    }

TTCN PDU: Assignment:[19] tcv_TmpAttachRe

(To search, click here and then press Ctrl+F)

    := PDU:
    {
      skipIndicator: '0000'B,
      gMMProtocolDiscriminator: '1000'B,
      msgType: '00000001'B,
      msNetworkCap:
      {
        iel: '02'O,
        value: 'E540'O
      },
      gprsCiphKeySeqNo:
      {
        spare1: '0'B,
        keySeq: '111'B
      },
      attachType:
      {
        for: '0'B,
        type: '001'B
      },
      drxParameter:
      {
        splitPGcycleCode: '00000111'B,
        cnDRXcoef: '0000'B,
        splitOnCCCH: '0'B,
        nonDRXtimer: '100'B
      },
      ptmsiORimsi:
      {
        iel: '08'O,
        iDigit1: '0000'B,
        oddEvenInd: '1'B,
        typeOfId: '001'B,
        otherDigits: '10100000003033'O
      },
      oldRAI:
      {
        plmn: '00F110'O,
        lac: 'FFFE'O,
        rac: '05'O
      },
      msRadioAccessCap:
      {
        iel: '0B'O,
        value: '15F38233542A332644A198'O
      },
      oldPTMSI_Signature: OMIT,
      readyTimer:
      {
        iei: '00010111'B,
        unit: '000'B,
        value: '10110'B
      },
      tmsiStatus: OMIT
    }

TTCN PDU: RRC_DataInd

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      rB_Id: 3,
      ch: OMIT,
      sapId: OMIT,
      cN_Domain: 1,
      start: '00000000000000000010'B,
      msg: PDU:
      {
        skipIndicator: '0000'B,
        gMMProtocolDiscriminator: '1000'B,
        msgType: '00000001'B,
        msNetworkCap:
        {
          iel: '02'O,
          value: 'E540'O
        },
        gprsCiphKeySeqNo:
        {
          spare1: '0'B,
          keySeq: '111'B
        },
        attachType:
        {
          for: '0'B,
          type: '001'B
        },
        drxParameter:
        {
          splitPGcycleCode: '00000111'B,
          cnDRXcoef: '0000'B,
          splitOnCCCH: '0'B,
          nonDRXtimer: '100'B
        },
        ptmsiORimsi:
        {
          iel: '08'O,
          iDigit1: '0000'B,
          oddEvenInd: '1'B,
          typeOfId: '001'B,
          otherDigits: '10100000003033'O
        },
        oldRAI:
        {
          plmn: '00F110'O,
          lac: 'FFFE'O,
          rac: '05'O
        },
        msRadioAccessCap:
        {
          iel: '0B'O,
          value: '15F38233542A332644A198'O
        },
        oldPTMSI_Signature: OMIT,
        readyTimer:
        {
          iei: '00010111'B,
          unit: '000'B,
          value: '10110'B
        },
        tmsiStatus: OMIT
      }
    }

TTCN PDU: Assignment:[3] tcv_AuthRs

(To search, click here and then press Ctrl+F)

    := PDU:
    {
      skipIndicator: '0000'B,
      mMProtocolDiscriminator: '0101'B,
      msgType: '01010100'B,
      authRsp: '01010101010001000111011101100110'B,
      authRspExt:
      {
        iei: '00100001'B,
        iel: '04'O,
        rES: '00010001000000000011001100100010'B
      }
    }

TTCN PDU: RRC_DataInd

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      rB_Id: 3,
      ch: OMIT,
      sapId: OMIT,
      cN_Domain: 0,
      start: OMIT,
      msg: PDU:
      {
        skipIndicator: '0000'B,
        mMProtocolDiscriminator: '0101'B,
        msgType: '01010100'B,
        authRsp: '01010101010001000111011101100110'B,
        authRspExt:
        {
          iei: '00100001'B,
          iel: '04'O,
          rES: '00010001000000000011001100100010'B
        }
      }
    }

TTCN PDU: CRLC_SecurityMode_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      rlcSecurityInfo:
      {
        cn_DomainIdentity: cs_domain,
        startValue: '00000000000000000000'B,
        cipheringKey: OMIT,
        integrityKey: '01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100'B,
        gsmCipheringKey: OMIT
      }
    }

TTCN PDU: CRLC_SetRRC_MessageSN_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: 0
      ],
      count_I_LSB_UL: OMIT,
      count_I_LSB_DL: 0
    }

TTCN PDU: CRLC_SetRRC_MessageSN_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 1
      ],
      count_I_LSB_UL: OMIT,
      count_I_LSB_DL: 0
    }

TTCN PDU: CRLC_SetRRC_MessageSN_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 2
      ],
      count_I_LSB_UL: OMIT,
      count_I_LSB_DL: 0
    }

TTCN PDU: CRLC_SetRRC_MessageSN_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 3
      ],
      count_I_LSB_UL: OMIT,
      count_I_LSB_DL: 0
    }

TTCN PDU: CRLC_SetRRC_MessageSN_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 4
      ],
      count_I_LSB_UL: OMIT,
      count_I_LSB_DL: 0
    }

TTCN PDU: CRLC_Integrity_Activate_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      cn_DomainIdentity: cs_domain,
      integrityActivationInfo:
      [
        integrityProtectionModeInfo:
        {
          integrityProtectionModeCommand:
          [
            startIntegrityProtection:
            {
              integrityProtInitNumber: '00001111000011110000111100001111'B
            }
          ],
          integrityProtectionAlgorithm: uia1
        }
      ]
    }

TTCN PDU: CRLC_Integrity_Activate_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      cn_DomainIdentity: cs_domain,
      integrityActivationInfo:
      [
        ul_IntegProtActivationInfo:
        [
          {
            rb_Identity: 2,
            rrc_MessageSequenceNumber: 0
          }
        ]
      ]
    }

TTCN PDU: RLC_AM_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 2
      ],
      confirmationRequest:
      [
        noConfirmationRequest: NULL
      ],
      aM_message:
      [
        dL_DCCH_Message: PDU:
        {
          integrityCheckInfo:
          {
            messageAuthenticationCode: '00010001001100011010010000011001'B,
            rrc_MessageSequenceNumber: 1
          },
          message:
          [
            securityModeCommand:
            [
              r3:
              {
                securityModeCommand_r3:
                {
                  rrc_TransactionIdentifier: 0,
                  securityCapability:
                  {
                    cipheringAlgorithmCap: '0000000000000011'B,
                    integrityProtectionAlgorithmCap: '0000000000000010'B
                  },
                  cipheringModeInfo: OMIT,
                  integrityProtectionModeInfo:
                  {
                    integrityProtectionModeCommand:
                    [
                      startIntegrityProtection:
                      {
                        integrityProtInitNumber: '00001111000011110000111100001111'B
                      }
                    ],
                    integrityProtectionAlgorithm: uia1
                  },
                  cn_DomainIdentity: cs_domain,
                  ue_SystemSpecificSecurityCap: OMIT
                },
                laterNonCriticalExtensions: OMIT
              }
            ]
          ]
        }
      ]
    }

TTCN PDU: RLC_AM_DATA_IND

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 2
      ],
      integrityResult:
      [
        integrityUsed: i_pass
      ],
      aM_message:
      [
        uL_DCCH_Message: PDU:
        {
          integrityCheckInfo:
          {
            messageAuthenticationCode: '10001011001000110111110011100010'B,
            rrc_MessageSequenceNumber: 1
          },
          message:
          [
            securityModeComplete:
            {
              rrc_TransactionIdentifier: 0,
              ul_IntegProtActivationInfo:
              {
                rrc_MessageSequenceNumberList:
                [
                  0,
                  0,
                  0,
                  0,
                  0
                ]
              },
              rb_UL_CiphActivationTimeInfo: OMIT,
              laterNonCriticalExtensions: OMIT
            }
          ]
        }
      ]
    }

TTCN PDU: CRLC_Integrity_Activate_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      cn_DomainIdentity: cs_domain,
      integrityActivationInfo:
      [
        ul_IntegProtActivationInfo:
        [
          {
            rb_Identity: 0,
            rrc_MessageSequenceNumber: 0
          },

          {
            rb_Identity: 1,
            rrc_MessageSequenceNumber: 0
          },

          {
            rb_Identity: 3,
            rrc_MessageSequenceNumber: 0
          },

          {
            rb_Identity: 4,
            rrc_MessageSequenceNumber: 0
          }
        ]
      ]
    }

TTCN PDU: RRC_DataReq

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      rB_Id: 3,
      ch: OMIT,
      sapId: OMIT,
      cN_Domain: 0,
      msg: PDU:
      {
        skipIndicator: '0000'B,
        mMProtocolDiscriminator: '0101'B,
        msgType: '00000010'B,
        locAreaId:
        {
          plmn: '00F210'O,
          lac: '0001'O
        },
        mobileId:
        {
          iei: '00010111'B,
          iel: '05'O,
          iDigit1: '1111'B,
          oddEvenInd: '0'B,
          typeOfId: '100'B,
          otherDigits: '11223344'O
        },
        followOnProceed: '10100001'B,
        cTSPerm: '10100010'B,
        equivalentPLMN: OMIT
      }
    }

TTCN PDU: RRC_DataInd

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      rB_Id: 3,
      ch: OMIT,
      sapId: OMIT,
      cN_Domain: 0,
      start: OMIT,
      msg: PDU:
      {
        skipIndicator: '0000'B,
        mMProtocolDiscriminator: '0101'B,
        msgType: '10011011'B
      }
    }

TTCN PDU: RRC_DataReq

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      rB_Id: 3,
      ch: OMIT,
      sapId: OMIT,
      cN_Domain: 1,
      msg: PDU:
      {
        skipIndicator: '0000'B,
        gMMProtocolDiscriminator: '1000'B,
        msgType: '00010010'B,
        imeisvReq:
        {
          spare1: '0'B,
          value: '000'B
        },
        ciphAlgorithm:
        {
          spare1: '0'B,
          algorithm: '001'B
        },
        acRefNo:
        {
          value: '0011'B
        },
        forceToStandby:
        {
          spare: '0'B,
          value: '000'B
        },
        authRand:
        {
          iei: '00100001'B,
          randValue: '01010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101'B
        },
        gprsCiphKeySeqNo:
        {
          iei: '1000'B,
          spare1: '0'B,
          keySeq: '000'B
        },
        aUTN:
        {
          iei: '00101000'B,
          iel: '10'O,
          aUTN: '01100110000100010000000000110011001000101101110100000000000000000101010101000100011101110110011000010001000000000011001100100010'B
        }
      }
    }

TTCN PDU: Assignment:[3] tcv_TmpAuthAndCiphRs

(To search, click here and then press Ctrl+F)

    := PDU:
    {
      skipIndicator: '0000'B,
      gMMProtocolDiscriminator: '1000'B,
      msgType: '00010011'B,
      spare4: '0000'B,
      acRefNo:
      {
        value: '0011'B
      },
      authRsp:
      {
        iei: '00100010'B,
        value: '01010101010001000111011101100110'B
      },
      imeisv: OMIT,
      authRspExt:
      {
        iei: '00101001'B,
        iel: '04'O,
        rES: '00010001000000000011001100100010'B
      }
    }

TTCN PDU: RRC_DataInd

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      rB_Id: 3,
      ch: OMIT,
      sapId: OMIT,
      cN_Domain: 1,
      start: OMIT,
      msg: PDU:
      {
        skipIndicator: '0000'B,
        gMMProtocolDiscriminator: '1000'B,
        msgType: '00010011'B,
        spare4: '0000'B,
        acRefNo:
        {
          value: '0011'B
        },
        authRsp:
        {
          iei: '00100010'B,
          value: '01010101010001000111011101100110'B
        },
        imeisv: OMIT,
        authRspExt:
        {
          iei: '00101001'B,
          iel: '04'O,
          rES: '00010001000000000011001100100010'B
        }
      }
    }

TTCN PDU: CRLC_RRC_MessageSN_CNF

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 0
      ],
      count_I_MSB_UL: 0,
      count_I_LSB_UL: 0,
      count_I_MSB_DL: 0,
      count_I_LSB_DL: 0
    }

TTCN PDU: CRLC_RRC_MessageSN_CNF

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 1
      ],
      count_I_MSB_UL: 0,
      count_I_LSB_UL: 0,
      count_I_MSB_DL: 0,
      count_I_LSB_DL: 0
    }

TTCN PDU: CRLC_RRC_MessageSN_CNF

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 2
      ],
      count_I_MSB_UL: 0,
      count_I_LSB_UL: 1,
      count_I_MSB_DL: 0,
      count_I_LSB_DL: 1
    }

TTCN PDU: CRLC_RRC_MessageSN_CNF

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 3
      ],
      count_I_MSB_UL: 0,
      count_I_LSB_UL: 2,
      count_I_MSB_DL: 0,
      count_I_LSB_DL: 2
    }

TTCN PDU: CRLC_RRC_MessageSN_CNF

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 4
      ],
      count_I_MSB_UL: 0,
      count_I_LSB_UL: 0,
      count_I_MSB_DL: 0,
      count_I_LSB_DL: 0
    }

TTCN PDU: CRLC_SecurityMode_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      rlcSecurityInfo:
      {
        cn_DomainIdentity: ps_domain,
        startValue: '00000000000000000000'B,
        cipheringKey: OMIT,
        integrityKey: '01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100'B,
        gsmCipheringKey: OMIT
      }
    }

TTCN PDU: CRLC_Integrity_Activate_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      cn_DomainIdentity: ps_domain,
      integrityActivationInfo:
      [
        integrityProtectionModeInfo:
        {
          integrityProtectionModeCommand:
          [
            modify:
            {
              dl_IntegrityProtActivationInfo:
              {
                rrc_MessageSequenceNumberList:
                [
                  0,
                  0,
                  1,
                  2,
                  0
                ]
              }
            }
          ],
          integrityProtectionAlgorithm: uia1
        }
      ]
    }

TTCN PDU: CRLC_Integrity_Activate_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      cn_DomainIdentity: ps_domain,
      integrityActivationInfo:
      [
        ul_IntegProtActivationInfo:
        [
          {
            rb_Identity: 2,
            rrc_MessageSequenceNumber: 1
          }
        ]
      ]
    }

TTCN PDU: RLC_AM_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 2
      ],
      confirmationRequest:
      [
        noConfirmationRequest: NULL
      ],
      aM_message:
      [
        dL_DCCH_Message: PDU:
        {
          integrityCheckInfo:
          {
            messageAuthenticationCode: '00100001110110000101111100011100'B,
            rrc_MessageSequenceNumber: 2
          },
          message:
          [
            securityModeCommand:
            [
              r3:
              {
                securityModeCommand_r3:
                {
                  rrc_TransactionIdentifier: 0,
                  securityCapability:
                  {
                    cipheringAlgorithmCap: '0000000000000011'B,
                    integrityProtectionAlgorithmCap: '0000000000000010'B
                  },
                  cipheringModeInfo: OMIT,
                  integrityProtectionModeInfo:
                  {
                    integrityProtectionModeCommand:
                    [
                      modify:
                      {
                        dl_IntegrityProtActivationInfo:
                        {
                          rrc_MessageSequenceNumberList:
                          [
                            0,
                            0,
                            1,
                            2,
                            0
                          ]
                        }
                      }
                    ],
                    integrityProtectionAlgorithm: uia1
                  },
                  cn_DomainIdentity: ps_domain,
                  ue_SystemSpecificSecurityCap: OMIT
                },
                laterNonCriticalExtensions: OMIT
              }
            ]
          ]
        }
      ]
    }

TTCN PDU: RLC_AM_DATA_IND

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 2
      ],
      integrityResult:
      [
        integrityUsed: i_pass
      ],
      aM_message:
      [
        uL_DCCH_Message: PDU:
        {
          integrityCheckInfo:
          {
            messageAuthenticationCode: '11100000000110011010110001001011'B,
            rrc_MessageSequenceNumber: 2
          },
          message:
          [
            securityModeComplete:
            {
              rrc_TransactionIdentifier: 0,
              ul_IntegProtActivationInfo:
              {
                rrc_MessageSequenceNumberList:
                [
                  5,
                  1,
                  2,
                  3,
                  1
                ]
              },
              rb_UL_CiphActivationTimeInfo: OMIT,
              laterNonCriticalExtensions: OMIT
            }
          ]
        }
      ]
    }

TTCN PDU: CRLC_Integrity_Activate_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      cn_DomainIdentity: ps_domain,
      integrityActivationInfo:
      [
        ul_IntegProtActivationInfo:
        [
          {
            rb_Identity: 0,
            rrc_MessageSequenceNumber: 5
          },

          {
            rb_Identity: 1,
            rrc_MessageSequenceNumber: 1
          },

          {
            rb_Identity: 3,
            rrc_MessageSequenceNumber: 3
          },

          {
            rb_Identity: 4,
            rrc_MessageSequenceNumber: 1
          }
        ]
      ]
    }

TTCN PDU: RRC_DataReq

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      rB_Id: 3,
      ch: OMIT,
      sapId: OMIT,
      cN_Domain: 1,
      msg: PDU:
      {
        skipIndicator: '0000'B,
        gMMProtocolDiscriminator: '1000'B,
        msgType: '00000010'B,
        forceToStandby:
        {
          spare: '0'B,
          value: '000'B
        },
        attachResult:
        {
          spare: '0'B,
          result: '001'B
        },
        periodicRAupdateTimer:
        {
          unit: '111'B,
          value: '00000'B
        },
        spare: '0000'B,
        radioPrioSMS:
        {
          spare: '0'B,
          value: '100'B
        },
        rai:
        {
          plmn: '00F210'O,
          lac: '0001'O,
          rac: '05'O
        },
        ptmsiSignature:
        {
          iei: '00011001'B,
          value: 'AB1234'O
        },
        negReadyTimer: OMIT,
        allocatedPTMSI:
        {
          iei: '00011000'B,
          iel: '05'O,
          iDigit1: '1111'B,
          oddEvenInd: '0'B,
          typeOfId: '100'B,
          otherDigits: '12345678'O
        },
        msIdentity: OMIT,
        gmmCause: OMIT,
        t3302Value: OMIT,
        cellNotification: OMIT,
        equivalentPLMN: OMIT
      }
    }

TTCN PDU: RRC_DataInd

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      rB_Id: 3,
      ch: OMIT,
      sapId: OMIT,
      cN_Domain: 1,
      start: OMIT,
      msg: PDU:
      {
        skipIndicator: '0000'B,
        gMMProtocolDiscriminator: '1000'B,
        msgType: '00000011'B
      }
    }

TTCN PDU: RLC_UM_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 1
      ],
      uM_message:
      [
        dL_DCCH_Message: PDU:
        {
          integrityCheckInfo:
          {
            messageAuthenticationCode: '11101100100111000001011111010011'B,
            rrc_MessageSequenceNumber: 1
          },
          message:
          [
            rrcConnectionRelease:
            [
              r3:
              {
                rrcConnectionRelease_r3:
                {
                  rrc_TransactionIdentifier: 0,
                  n_308: 1,
                  releaseCause: normalEvent,
                  rplmn_information: OMIT
                },
                laterNonCriticalExtensions: OMIT
              }
            ]
          ]
        }
      ],
      specialLI: GcFALSE
    }

TTCN PDU: RLC_UM_DATA_IND

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 1
      ],
      integrityResult:
      [
        integrityUsed: i_pass
      ],
      uM_message:
      [
        uL_DCCH_Message: PDU:
        {
          integrityCheckInfo:
          {
            messageAuthenticationCode: '11110111111000101100001011001110'B,
            rrc_MessageSequenceNumber: 1
          },
          message:
          [
            rrcConnectionReleaseComplete:
            {
              rrc_TransactionIdentifier: 0,
              errorIndication: OMIT,
              laterNonCriticalExtensions: OMIT
            }
          ]
        }
      ]
    }

TTCN PDU: RLC_UM_DATA_IND

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 1
      ],
      integrityResult:
      [
        integrityUsed: i_pass
      ],
      uM_message:
      [
        uL_DCCH_Message: PDU:
        {
          integrityCheckInfo:
          {
            messageAuthenticationCode: '10111001101000110000011111000000'B,
            rrc_MessageSequenceNumber: 2
          },
          message:
          [
            rrcConnectionReleaseComplete:
            {
              rrc_TransactionIdentifier: 0,
              errorIndication: OMIT,
              laterNonCriticalExtensions: OMIT
            }
          ]
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 1
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 2
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 3
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 4
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 1
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          sS_rlc_Info:
          {
            sS_ul_RLC_Mode:
            [
              dl_UM_RLC_Mode: NULL
            ],
            sS_dl_RLC_Mode:
            {
              dl_PayloadSize: 136,
              dl_RLCModeInfo:
              [
                ul_UM_RLC_Mode:
                {
                  transmissionRLC_Discard:
                  [
                    timerBasedNoExplicit: dt100
                  ]
                }
              ]
            }
          },
          rB_LogCH_Mapping:
          {
            uLlogicalChannelIdentity: 1,
            dLlogicalChannelIdentity: 1,
            logicalChannelType: OMIT,
            cn_DomainIdentity: OMIT
          }
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 2
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          sS_rlc_Info:
          {
            sS_ul_RLC_Mode:
            [
              dl_AM_RLC_Mode:
              {
                inSequenceDelivery: GcTRUE,
                receivingWindowSize: rw32,
                dl_RLC_StatusInfo:
                {
                  timerStatusProhibit: tsp200,
                  timerEPC: OMIT,
                  missingPDU_Indicator: GcTRUE,
                  timerStatusPeriodic: OMIT
                }
              }
            ],
            sS_dl_RLC_Mode:
            {
              dl_PayloadSize: 128,
              dl_RLCModeInfo:
              [
                ul_AM_RLC_Mode:
                {
                  transmissionRLC_Discard:
                  [
                    noDiscard: dat15
                  ],
                  transmissionWindowSize: tw32,
                  timerRST: tr500,
                  max_RST: rst1,
                  pollingInfo:
                  {
                    timerPollProhibit: tpp200,
                    timerPoll: tp200,
                    poll_PDU: OMIT,
                    poll_SDU: sdu1,
                    lastTransmissionPDU_Poll: GcTRUE,
                    lastRetransmissionPDU_Poll: GcTRUE,
                    pollWindow: pw99,
                    timerPollPeriodic: OMIT
                  }
                }
              ]
            }
          },
          rB_LogCH_Mapping:
          {
            uLlogicalChannelIdentity: 2,
            dLlogicalChannelIdentity: 2,
            logicalChannelType: OMIT,
            cn_DomainIdentity: OMIT
          }
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 3
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          sS_rlc_Info:
          {
            sS_ul_RLC_Mode:
            [
              dl_AM_RLC_Mode:
              {
                inSequenceDelivery: GcTRUE,
                receivingWindowSize: rw32,
                dl_RLC_StatusInfo:
                {
                  timerStatusProhibit: tsp200,
                  timerEPC: OMIT,
                  missingPDU_Indicator: GcTRUE,
                  timerStatusPeriodic: OMIT
                }
              }
            ],
            sS_dl_RLC_Mode:
            {
              dl_PayloadSize: 128,
              dl_RLCModeInfo:
              [
                ul_AM_RLC_Mode:
                {
                  transmissionRLC_Discard:
                  [
                    noDiscard: dat15
                  ],
                  transmissionWindowSize: tw32,
                  timerRST: tr500,
                  max_RST: rst1,
                  pollingInfo:
                  {
                    timerPollProhibit: tpp200,
                    timerPoll: tp200,
                    poll_PDU: OMIT,
                    poll_SDU: sdu1,
                    lastTransmissionPDU_Poll: GcTRUE,
                    lastRetransmissionPDU_Poll: GcTRUE,
                    pollWindow: pw99,
                    timerPollPeriodic: OMIT
                  }
                }
              ]
            }
          },
          rB_LogCH_Mapping:
          {
            uLlogicalChannelIdentity: 3,
            dLlogicalChannelIdentity: 3,
            logicalChannelType: OMIT,
            cn_DomainIdentity: OMIT
          }
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 4
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          sS_rlc_Info:
          {
            sS_ul_RLC_Mode:
            [
              dl_AM_RLC_Mode:
              {
                inSequenceDelivery: GcTRUE,
                receivingWindowSize: rw32,
                dl_RLC_StatusInfo:
                {
                  timerStatusProhibit: tsp200,
                  timerEPC: OMIT,
                  missingPDU_Indicator: GcTRUE,
                  timerStatusPeriodic: OMIT
                }
              }
            ],
            sS_dl_RLC_Mode:
            {
              dl_PayloadSize: 128,
              dl_RLCModeInfo:
              [
                ul_AM_RLC_Mode:
                {
                  transmissionRLC_Discard:
                  [
                    noDiscard: dat15
                  ],
                  transmissionWindowSize: tw32,
                  timerRST: tr500,
                  max_RST: rst1,
                  pollingInfo:
                  {
                    timerPollProhibit: tpp200,
                    timerPoll: tp200,
                    poll_PDU: OMIT,
                    poll_SDU: sdu1,
                    lastTransmissionPDU_Poll: GcTRUE,
                    lastRetransmissionPDU_Poll: GcTRUE,
                    pollWindow: pw99,
                    timerPollPeriodic: OMIT
                  }
                }
              ]
            }
          },
          rB_LogCH_Mapping:
          {
            uLlogicalChannelIdentity: 4,
            dLlogicalChannelIdentity: 4,
            logicalChannelType: OMIT,
            cn_DomainIdentity: OMIT
          }
        }
      ]
    }

TTCN PDU: RLC_TR_DATA_IND

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: 0
      ],
      tM_message:
      [
        uL_CCCH_Message: PDU:
        {
          integrityCheckInfo: OMIT,
          message:
          [
            rrcConnectionRequest:
            {
              initialUE_Identity:
              [
                tmsi_and_LAI:
                {
                  tmsi: '00010001001000100011001101000100'B,
                  lai:
                  {
                    plmn_Identity:
                    {
                      mcc:
                      [
                        0,
                        0,
                        2
                      ],
                      mnc:
                      [
                        0,
                        1
                      ]
                    },
                    lac: '0000000000000001'B
                  }
                }
              ],
              establishmentCause: detach,
              protocolErrorIndicator: noError,
              measuredResultsOnRACH: OMIT,
              v3d0NonCriticalExtensions: OMIT
            }
          ]
        }
      ]
    }

TTCN PDU: RLC_UM_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: 0
      ],
      uM_message:
      [
        dL_CCCH_Message: PDU:
        {
          integrityCheckInfo: OMIT,
          message:
          [
            rrcConnectionSetup:
            [
              r3:
              {
                rrcConnectionSetup_r3:
                {
                  initialUE_Identity:
                  [
                    tmsi_and_LAI:
                    {
                      tmsi: '00010001001000100011001101000100'B,
                      lai:
                      {
                        plmn_Identity:
                        {
                          mcc:
                          [
                            0,
                            0,
                            2
                          ],
                          mnc:
                          [
                            0,
                            1
                          ]
                        },
                        lac: '0000000000000001'B
                      }
                    }
                  ],
                  rrc_TransactionIdentifier: 0,
                  activationTime: OMIT,
                  new_U_RNTI:
                  {
                    srnc_Identity: '000000000001'B,
                    s_RNTI: '00000000000000000001'B
                  },
                  new_c_RNTI: OMIT,
                  rrc_StateIndicator: cell_DCH,
                  utran_DRX_CycleLengthCoeff: 9,
                  capabilityUpdateRequirement:
                  {
                    ue_RadioCapabilityFDDUpdateRequirement: GcTRUE,
                    ue_RadioCapabilityTDDUpdateRequirement: GcFALSE,
                    systemSpecificCapUpdateReqList:
                    [
                      gsm
                    ]
                  },
                  srb_InformationSetupList:
                  [
                    {
                      rb_Identity: OMIT,
                      rlc_InfoChoice:
                      [
                        rlc_Info:
                        {
                          ul_RLC_Mode:
                          [
                            ul_UM_RLC_Mode:
                            {
                              transmissionRLC_Discard: OMIT
                            }
                          ],
                          dl_RLC_Mode:
                          [
                            dl_UM_RLC_Mode: NULL
                          ]
                        }
                      ],
                      rb_MappingInfo:
                      [
                        {
                          ul_LogicalChannelMappings:
                          [
                            oneLogicalChannel:
                            {
                              ul_TransportChannelType:
                              [
                                dch: 5
                              ],
                              logicalChannelIdentity: 1,
                              rlc_SizeList:
                              [
                                configured: NULL
                              ],
                              mac_LogicalChannelPriority: 1
                            }
                          ],
                          dl_LogicalChannelMappingList:
                          [
                            {
                              dl_TransportChannelType:
                              [
                                dch: 10
                              ],
                              logicalChannelIdentity: 1
                            }
                          ]
                        },

                        {
                          ul_LogicalChannelMappings:
                          [
                            oneLogicalChannel:
                            {
                              ul_TransportChannelType:
                              [
                                rach: NULL
                              ],
                              logicalChannelIdentity: 1,
                              rlc_SizeList:
                              [
                                explicitList:
                                [
                                  {
                                    rlc_SizeIndex: 1
                                  }
                                ]
                              ],
                              mac_LogicalChannelPriority: 1
                            }
                          ],
                          dl_LogicalChannelMappingList:
                          [
                            {
                              dl_TransportChannelType:
                              [
                                fach: NULL
                              ],
                              logicalChannelIdentity: 1
                            }
                          ]
                        }
                      ]
                    },

                    {
                      rb_Identity: OMIT,
                      rlc_InfoChoice:
                      [
                        rlc_Info:
                        {
                          ul_RLC_Mode:
                          [
                            ul_AM_RLC_Mode:
                            {
                              transmissionRLC_Discard:
                              [
                                noDiscard: dat15
                              ],
                              transmissionWindowSize: tw32,
                              timerRST: tr500,
                              max_RST: rst1,
                              pollingInfo:
                              {
                                timerPollProhibit: tpp200,
                                timerPoll: tp200,
                                poll_PDU: OMIT,
                                poll_SDU: sdu1,
                                lastTransmissionPDU_Poll: GcTRUE,
                                lastRetransmissionPDU_Poll: GcTRUE,
                                pollWindow: pw99,
                                timerPollPeriodic: OMIT
                              }
                            }
                          ],
                          dl_RLC_Mode:
                          [
                            dl_AM_RLC_Mode:
                            {
                              inSequenceDelivery: GcTRUE,
                              receivingWindowSize: rw32,
                              dl_RLC_StatusInfo:
                              {
                                timerStatusProhibit: tsp200,
                                timerEPC: OMIT,
                                missingPDU_Indicator: GcTRUE,
                                timerStatusPeriodic: OMIT
                              }
                            }
                          ]
                        }
                      ],
                      rb_MappingInfo:
                      [
                        {
                          ul_LogicalChannelMappings:
                          [
                            oneLogicalChannel:
                            {
                              ul_TransportChannelType:
                              [
                                dch: 5
                              ],
                              logicalChannelIdentity: 2,
                              rlc_SizeList:
                              [
                                configured: NULL
                              ],
                              mac_LogicalChannelPriority: 2
                            }
                          ],
                          dl_LogicalChannelMappingList:
                          [
                            {
                              dl_TransportChannelType:
                              [
                                dch: 10
                              ],
                              logicalChannelIdentity: 2
                            }
                          ]
                        },

                        {
                          ul_LogicalChannelMappings:
                          [
                            oneLogicalChannel:
                            {
                              ul_TransportChannelType:
                              [
                                rach: NULL
                              ],
                              logicalChannelIdentity: 2,
                              rlc_SizeList:
                              [
                                explicitList:
                                [
                                  {
                                    rlc_SizeIndex: 1
                                  }
                                ]
                              ],
                              mac_LogicalChannelPriority: 2
                            }
                          ],
                          dl_LogicalChannelMappingList:
                          [
                            {
                              dl_TransportChannelType:
                              [
                                fach: NULL
                              ],
                              logicalChannelIdentity: 2
                            }
                          ]
                        }
                      ]
                    },

                    {
                      rb_Identity: OMIT,
                      rlc_InfoChoice:
                      [
                        rlc_Info:
                        {
                          ul_RLC_Mode:
                          [
                            ul_AM_RLC_Mode:
                            {
                              transmissionRLC_Discard:
                              [
                                noDiscard: dat15
                              ],
                              transmissionWindowSize: tw32,
                              timerRST: tr500,
                              max_RST: rst1,
                              pollingInfo:
                              {
                                timerPollProhibit: tpp200,
                                timerPoll: tp200,
                                poll_PDU: OMIT,
                                poll_SDU: sdu1,
                                lastTransmissionPDU_Poll: GcTRUE,
                                lastRetransmissionPDU_Poll: GcTRUE,
                                pollWindow: pw99,
                                timerPollPeriodic: OMIT
                              }
                            }
                          ],
                          dl_RLC_Mode:
                          [
                            dl_AM_RLC_Mode:
                            {
                              inSequenceDelivery: GcTRUE,
                              receivingWindowSize: rw32,
                              dl_RLC_StatusInfo:
                              {
                                timerStatusProhibit: tsp200,
                                timerEPC: OMIT,
                                missingPDU_Indicator: GcTRUE,
                                timerStatusPeriodic: OMIT
                              }
                            }
                          ]
                        }
                      ],
                      rb_MappingInfo:
                      [
                        {
                          ul_LogicalChannelMappings:
                          [
                            oneLogicalChannel:
                            {
                              ul_TransportChannelType:
                              [
                                dch: 5
                              ],
                              logicalChannelIdentity: 3,
                              rlc_SizeList:
                              [
                                configured: NULL
                              ],
                              mac_LogicalChannelPriority: 3
                            }
                          ],
                          dl_LogicalChannelMappingList:
                          [
                            {
                              dl_TransportChannelType:
                              [
                                dch: 10
                              ],
                              logicalChannelIdentity: 3
                            }
                          ]
                        },

                        {
                          ul_LogicalChannelMappings:
                          [
                            oneLogicalChannel:
                            {
                              ul_TransportChannelType:
                              [
                                rach: NULL
                              ],
                              logicalChannelIdentity: 3,
                              rlc_SizeList:
                              [
                                explicitList:
                                [
                                  {
                                    rlc_SizeIndex: 1
                                  }
                                ]
                              ],
                              mac_LogicalChannelPriority: 3
                            }
                          ],
                          dl_LogicalChannelMappingList:
                          [
                            {
                              dl_TransportChannelType:
                              [
                                fach: NULL
                              ],
                              logicalChannelIdentity: 3
                            }
                          ]
                        }
                      ]
                    },

                    {
                      rb_Identity: OMIT,
                      rlc_InfoChoice:
                      [
                        rlc_Info:
                        {
                          ul_RLC_Mode:
                          [
                            ul_AM_RLC_Mode:
                            {
                              transmissionRLC_Discard:
                              [
                                noDiscard: dat15
                              ],
                              transmissionWindowSize: tw32,
                              timerRST: tr500,
                              max_RST: rst1,
                              pollingInfo:
                              {
                                timerPollProhibit: tpp200,
                                timerPoll: tp200,
                                poll_PDU: OMIT,
                                poll_SDU: sdu1,
                                lastTransmissionPDU_Poll: GcTRUE,
                                lastRetransmissionPDU_Poll: GcTRUE,
                                pollWindow: pw99,
                                timerPollPeriodic: OMIT
                              }
                            }
                          ],
                          dl_RLC_Mode:
                          [
                            dl_AM_RLC_Mode:
                            {
                              inSequenceDelivery: GcTRUE,
                              receivingWindowSize: rw32,
                              dl_RLC_StatusInfo:
                              {
                                timerStatusProhibit: tsp200,
                                timerEPC: OMIT,
                                missingPDU_Indicator: GcTRUE,
                                timerStatusPeriodic: OMIT
                              }
                            }
                          ]
                        }
                      ],
                      rb_MappingInfo:
                      [
                        {
                          ul_LogicalChannelMappings:
                          [
                            oneLogicalChannel:
                            {
                              ul_TransportChannelType:
                              [
                                dch: 5
                              ],
                              logicalChannelIdentity: 4,
                              rlc_SizeList:
                              [
                                configured: NULL
                              ],
                              mac_LogicalChannelPriority: 4
                            }
                          ],
                          dl_LogicalChannelMappingList:
                          [
                            {
                              dl_TransportChannelType:
                              [
                                dch: 10
                              ],
                              logicalChannelIdentity: 4
                            }
                          ]
                        },

                        {
                          ul_LogicalChannelMappings:
                          [
                            oneLogicalChannel:
                            {
                              ul_TransportChannelType:
                              [
                                rach: NULL
                              ],
                              logicalChannelIdentity: 4,
                              rlc_SizeList:
                              [
                                explicitList:
                                [
                                  {
                                    rlc_SizeIndex: 1
                                  }
                                ]
                              ],
                              mac_LogicalChannelPriority: 4
                            }
                          ],
                          dl_LogicalChannelMappingList:
                          [
                            {
                              dl_TransportChannelType:
                              [
                                fach: NULL
                              ],
                              logicalChannelIdentity: 4
                            }
                          ]
                        }
                      ]
                    }
                  ],
                  ul_CommonTransChInfo:
                  {
                    tfc_Subset: OMIT,
                    prach_TFCS: OMIT,
                    modeSpecificInfo:
                    [
                      fdd:
                      {
                        ul_TFCS:
                        [
                          normalTFCI_Signalling:
                          [
                            complete:
                            {
                              ctfcSize:
                              [
                                ctfc2Bit:
                                [
                                  {
                                    ctfc2: 0,
                                    powerOffsetInformation:
                                    {
                                      gainFactorInformation:
                                      [
                                        computedGainFactors: 0
                                      ],
                                      powerOffsetPp_m: OMIT
                                    }
                                  },

                                  {
                                    ctfc2: 1,
                                    powerOffsetInformation:
                                    {
                                      gainFactorInformation:
                                      [
                                        signalledGainFactors:
                                        {
                                          modeSpecificInfo:
                                          [
                                            fdd:
                                            {
                                              gainFactorBetaC: 11
                                            }
                                          ],
                                          gainFactorBetaD: 15,
                                          referenceTFC_ID: 0
                                        }
                                      ],
                                      powerOffsetPp_m: OMIT
                                    }
                                  }
                                ]
                              ]
                            }
                          ]
                        ]
                      }
                    ]
                  },
                  ul_AddReconfTransChInfoList:
                  [
                    {
                      ul_TransportChannelType: dch,
                      transportChannelIdentity: 5,
                      transportFormatSet:
                      [
                        dedicatedTransChTFS:
                        {
                          tti:
                          [
                            tti10:
                            [
                              {
                                rlc_Size:
                                [
                                  bitMode:
                                  [
                                    sizeType2:
                                    {
                                      part1: 2,
                                      part2: OMIT
                                    }
                                  ]
                                ],
                                numberOfTbSizeList:
                                [
                                  [
                                    zero: NULL
                                  ],

                                  [
                                    one: NULL
                                  ]
                                ],
                                logicalChannelList:
                                [
                                  allSizes: NULL
                                ]
                              }
                            ]
                          ],
                          semistaticTF_Information:
                          {
                            channelCodingType:
                            [
                              convolutional: third
                            ],
                            rateMatchingAttribute# 192 # crc_Size# crc16
                          }
                        }
                      ]
                    }
                  ]
                  # dl_CommonTransChInfo#
                  {
                    sccpch_TFCS# OMIT# modeSpecificInfo#
                    [
                      fdd#
                      {
                        dl_Parameters#
                        [
                          sameAsUL# NULL
                        ]
                      }
                    ]
                  }
                  # dl_AddReconfTransChInfoList#
                  [
                    {
                      dl_TransportChannelType# dch# dl_transportChannelIdentity# 10 # tfs_SignallingMode#
                      [
                        sameAsULTrCH#
                        {
                          ul_TransportChannelType# dch# ul_TransportChannelIdentity# 5
                        }
                      ]
                      # dch_QualityTarget#
                      {
                        bler_QualityValue# #20
                      }
                      # dummy# OMIT
                    }
                  ]
                  # frequencyInfo# OMIT# maxAllowedUL_TX_Power# OMIT# ul_ChannelRequirement#
                  [
                    ul_DPCH_Info#
                    {
                      ul_DPCH_PowerControlInfo#
                      [
                        fdd#
                        {
                          dpcch_PowerOffset# #40 # pc_Preamble# 1 # sRB_delay# 7 # powerControlAlgorithm#
                          [
                            algorithm1# 0
                          ]
                        }
                      ]
                      # modeSpecificInfo#
                      [
                        fdd#
                        {
                          scramblingCodeType# longSC# scramblingCode# 3000 # numberOfDPDCH# OMIT# spreadingFactor# sf64# tfci_Existence# GcTRUE # numberOfFBI_Bits# OMIT# puncturingLimit# pl1
                        }
                      ]
                    }
                  ]
                  # dl_CommonInformation#
                  {
                    dl_DPCH_InfoCommon#
                    {
                      cfnHandling#
                      [
                        initialise#
                        {
                          cfntargetsfnframeoffset# OMIT
                        }
                      ]
                      # modeSpecificInfo#
                      [
                        fdd#
                        {
                          dl_DPCH_PowerControlInfo#
                          {
                            modeSpecificInfo#
                            [
                              fdd#
                              {
                                dpc_Mode# singleTPC
                              }
                            ]
                          }
                          # powerOffsetPilot_pdpdch# 0 # dl_rate_matching_restriction# OMIT# spreadingFactorAndPilot#
                          [
                            sfd128# pb4
                          ]
                          # positionFixedOrFlexible# fixed# tfci_Existence# GcFALSE
                        }
                      ]
                    }
                    # modeSpecificInfo#
                    [
                      fdd#
                      {
                        defaultDPCH_OffsetValue# 0 # dpch_CompressedModeInfo# OMIT# tx_DiversityMode# noDiversity# ssdt_Information# OMIT
                      }
                    ]
                  }
                  # dl_InformationPerRL_List#
                  [
                    {
                      modeSpecificInfo#
                      [
                        fdd#
                        {
                          primaryCPICH_Info#
                          {
                            primaryScramblingCode# 250
                          }
                          # pdsch_SHO_DCH_Info# OMIT# pdsch_CodeMapping# OMIT
                        }
                      ]
                      # dl_DPCH_InfoPerRL#
                      [
                        fdd#
                        {
                          pCPICH_UsageForChannelEst# mayBeUsed# dpch_FrameOffset# 0 # secondaryCPICH_Info# OMIT# dl_ChannelisationCodeList#
                          [
                            {
                              secondaryScramblingCode# 1 # sf_AndCodeNumber#
                              [
                                sf128# 0
                              ]
                              # scramblingCodeChange# noCodeChange
                            }
                          ]
                          # tpc_CombinationIndex# 0 # ssdt_CellIdentity# OMIT# closedLoopTimingAdjMode# OMIT
                        }
                      ]
                      # sccpch_InfoforFACH# OMIT
                    }
                  ]
                }
                # laterNonCriticalExtensions# OMIT
              }
            ]
          ]
        }
      ]
      # specialLI# GcTRUE
    }

TTCN PDU: RLC_AM_DATA_IND

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 2
      ],
      integrityResult:
      [
        integrityUsed: i_pass
      ],
      aM_message:
      [
        uL_DCCH_Message: PDU:
        {
          integrityCheckInfo: OMIT,
          message:
          [
            rrcConnectionSetupComplete:
            {
              rrc_TransactionIdentifier: 0,
              startList:
              [
                {
                  cn_DomainIdentity: ps_domain,
                  start_Value: '00000000000000000010'B
                },

                {
                  cn_DomainIdentity: cs_domain,
                  start_Value: '00000000000000000010'B
                }
              ],
              ue_RadioAccessCapability:
              {
                accessStratumReleaseIndicator: r99,
                pdcp_Capability:
                {
                  losslessSRNS_RelocationSupport: GcFALSE,
                  supportForRfc2507:
                  [
                    notSupported: NULL
                  ]
                },
                rlc_Capability:
                {
                  totalRLC_AM_BufferSize: kb50,
                  maximumRLC_WindowSize: mws2047,
                  maximumAM_EntityNumber: am6
                },
                transportChannelCapability:
                {
                  dl_TransChCapability:
                  {
                    maxNoBitsReceived: b8960,
                    maxConvCodeBitsReceived: b1280,
                    turboDecodingSupport:
                    [
                      supported: b8960
                    ],
                    maxSimultaneousTransChs: e8,
                    maxSimultaneousCCTrCH_Count: 1,
                    maxReceivedTransportBlocks: tb32,
                    maxNumberOfTFC: tfc128,
                    maxNumberOfTF: tf64
                  },
                  ul_TransChCapability:
                  {
                    maxNoBitsTransmitted: b3840,
                    maxConvCodeBitsTransmitted: b1280,
                    turboEncodingSupport:
                    [
                      supported: b3840
                    ],
                    maxSimultaneousTransChs: e8,
                    modeSpecificInfo:
                    [
                      fdd: NULL
                    ],
                    maxTransmittedBlocks: tb32,
                    maxNumberOfTFC: tfc64,
                    maxNumberOfTF: tf32
                  }
                },
                rf_Capability:
                {
                  fddRF_Capability:
                  {
                    ue_PowerClass: 4,
                    txRxFrequencySeparation: mhz190
                  },
                  tddRF_Capability: OMIT
                },
                physicalChannelCapability:
                {
                  fddPhysChCapability:
                  {
                    downlinkPhysChCapability:
                    {
                      maxNoDPCH_PDSCH_Codes: 1,
                      maxNoPhysChBitsReceived: b9600,
                      supportForSF_512: GcFALSE,
                      supportOfPDSCH: GcFALSE,
                      simultaneousSCCPCH_DPCH_Reception:
                      [
                        notSupported: NULL
                      ]
                    },
                    uplinkPhysChCapability:
                    {
                      maxNoDPDCH_BitsTransmitted: b4800,
                      supportOfPCPCH: GcFALSE
                    }
                  },
                  tddPhysChCapability: OMIT
                },
                ue_MultiModeRAT_Capability:
                {
                  multiRAT_CapabilityList:
                  {
                    supportOfGSM: GcFALSE,
                    supportOfMulticarrier: GcFALSE
                  },
                  multiModeCapability: fdd
                },
                securityCapability:
                {
                  cipheringAlgorithmCap: '0000000000000011'B,
                  integrityProtectionAlgorithmCap: '0000000000000010'B
                },
                ue_positioning_Capability:
                {
                  standaloneLocMethodsSupported: GcFALSE,
                  ue_BasedOTDOA_Supported: GcFALSE,
                  networkAssistedGPS_Supported: noNetworkAssistedGPS,
                  supportForUE_GPS_TimingOfCellFrames: GcFALSE,
                  supportForIPDL: GcFALSE
                },
                measurementCapability:
                {
                  downlinkCompressedMode:
                  {
                    fdd_Measurements: GcTRUE,
                    tdd_Measurements: OMIT,
                    gsm_Measurements:
                    {
                      gsm900: GcTRUE,
                      dcs1800: GcTRUE,
                      gsm1900: GcTRUE
                    },
                    multiCarrierMeasurements: GcFALSE
                  },
                  uplinkCompressedMode:
                  {
                    fdd_Measurements: GcTRUE,
                    tdd_Measurements: OMIT,
                    gsm_Measurements:
                    {
                      gsm900: GcTRUE,
                      dcs1800: GcTRUE,
                      gsm1900: GcTRUE
                    },
                    multiCarrierMeasurements: GcFALSE
                  }
                }
              },
              ue_RATSpecificCapability: OMIT,
              v370NonCriticalExtensions: OMIT
            }
          ]
        }
      ]
    }

TTCN PDU: RRC_DataInd

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      rB_Id: 3,
      ch: OMIT,
      sapId: OMIT,
      cN_Domain: 1,
      start: '00000000000000000010'B,
      msg: PDU:
      {
        skipIndicator: '0000'B,
        gMMProtocolDiscriminator: '1000'B,
        msgType: '00000101'B,
        spare4: '0000'B,
        detachType:
        {
          powOff: '1'B,
          type: '001'B
        },
        ptmsi:
        {
          iei: '00011000'B,
          iel: '05'O,
          iDigit1: '1111'B,
          oddEvenInd: '0'B,
          typeOfId: '100'B,
          otherDigits: '12345678'O
        },
        ptmsiSignature:
        {
          iei: '00011001'B,
          iel: '03'O,
          value: 'AB1234'O
        }
      }
    }

TTCN PDU: RLC_UM_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 1
      ],
      uM_message:
      [
        dL_DCCH_Message: PDU:
        {
          integrityCheckInfo: OMIT,
          message:
          [
            rrcConnectionRelease:
            [
              r3:
              {
                rrcConnectionRelease_r3:
                {
                  rrc_TransactionIdentifier: 0,
                  n_308: 1,
                  releaseCause: normalEvent,
                  rplmn_information: OMIT
                },
                laterNonCriticalExtensions: OMIT
              }
            ]
          ]
        }
      ],
      specialLI: GcFALSE
    }

TTCN PDU: RLC_UM_DATA_IND

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 1
      ],
      integrityResult:
      [
        integrityUsed: i_pass
      ],
      uM_message:
      [
        uL_DCCH_Message: PDU:
        {
          integrityCheckInfo: OMIT,
          message:
          [
            rrcConnectionReleaseComplete:
            {
              rrc_TransactionIdentifier: 0,
              errorIndication: OMIT,
              laterNonCriticalExtensions: OMIT
            }
          ]
        }
      ]
    }

TTCN PDU: RLC_UM_DATA_IND

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 1
      ],
      integrityResult:
      [
        integrityUsed: i_pass
      ],
      uM_message:
      [
        uL_DCCH_Message: PDU:
        {
          integrityCheckInfo: OMIT,
          message:
          [
            rrcConnectionReleaseComplete:
            {
              rrc_TransactionIdentifier: 0,
              errorIndication: OMIT,
              laterNonCriticalExtensions: OMIT
            }
          ]
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 1
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 2
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 3
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 4
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 1
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          sS_rlc_Info:
          {
            sS_ul_RLC_Mode:
            [
              dl_UM_RLC_Mode: NULL
            ],
            sS_dl_RLC_Mode:
            {
              dl_PayloadSize: 136,
              dl_RLCModeInfo:
              [
                ul_UM_RLC_Mode:
                {
                  transmissionRLC_Discard:
                  [
                    timerBasedNoExplicit: dt100
                  ]
                }
              ]
            }
          },
          rB_LogCH_Mapping:
          {
            uLlogicalChannelIdentity: 1,
            dLlogicalChannelIdentity: 1,
            logicalChannelType: OMIT,
            cn_DomainIdentity: OMIT
          }
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 2
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          sS_rlc_Info:
          {
            sS_ul_RLC_Mode:
            [
              dl_AM_RLC_Mode:
              {
                inSequenceDelivery: GcTRUE,
                receivingWindowSize: rw32,
                dl_RLC_StatusInfo:
                {
                  timerStatusProhibit: tsp200,
                  timerEPC: OMIT,
                  missingPDU_Indicator: GcTRUE,
                  timerStatusPeriodic: OMIT
                }
              }
            ],
            sS_dl_RLC_Mode:
            {
              dl_PayloadSize: 128,
              dl_RLCModeInfo:
              [
                ul_AM_RLC_Mode:
                {
                  transmissionRLC_Discard:
                  [
                    noDiscard: dat15
                  ],
                  transmissionWindowSize: tw32,
                  timerRST: tr500,
                  max_RST: rst1,
                  pollingInfo:
                  {
                    timerPollProhibit: tpp200,
                    timerPoll: tp200,
                    poll_PDU: OMIT,
                    poll_SDU: sdu1,
                    lastTransmissionPDU_Poll: GcTRUE,
                    lastRetransmissionPDU_Poll: GcTRUE,
                    pollWindow: pw99,
                    timerPollPeriodic: OMIT
                  }
                }
              ]
            }
          },
          rB_LogCH_Mapping:
          {
            uLlogicalChannelIdentity: 2,
            dLlogicalChannelIdentity: 2,
            logicalChannelType: OMIT,
            cn_DomainIdentity: OMIT
          }
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 3
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          sS_rlc_Info:
          {
            sS_ul_RLC_Mode:
            [
              dl_AM_RLC_Mode:
              {
                inSequenceDelivery: GcTRUE,
                receivingWindowSize: rw32,
                dl_RLC_StatusInfo:
                {
                  timerStatusProhibit: tsp200,
                  timerEPC: OMIT,
                  missingPDU_Indicator: GcTRUE,
                  timerStatusPeriodic: OMIT
                }
              }
            ],
            sS_dl_RLC_Mode:
            {
              dl_PayloadSize: 128,
              dl_RLCModeInfo:
              [
                ul_AM_RLC_Mode:
                {
                  transmissionRLC_Discard:
                  [
                    noDiscard: dat15
                  ],
                  transmissionWindowSize: tw32,
                  timerRST: tr500,
                  max_RST: rst1,
                  pollingInfo:
                  {
                    timerPollProhibit: tpp200,
                    timerPoll: tp200,
                    poll_PDU: OMIT,
                    poll_SDU: sdu1,
                    lastTransmissionPDU_Poll: GcTRUE,
                    lastRetransmissionPDU_Poll: GcTRUE,
                    pollWindow: pw99,
                    timerPollPeriodic: OMIT
                  }
                }
              ]
            }
          },
          rB_LogCH_Mapping:
          {
            uLlogicalChannelIdentity: 3,
            dLlogicalChannelIdentity: 3,
            logicalChannelType: OMIT,
            cn_DomainIdentity: OMIT
          }
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 4
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          sS_rlc_Info:
          {
            sS_ul_RLC_Mode:
            [
              dl_AM_RLC_Mode:
              {
                inSequenceDelivery: GcTRUE,
                receivingWindowSize: rw32,
                dl_RLC_StatusInfo:
                {
                  timerStatusProhibit: tsp200,
                  timerEPC: OMIT,
                  missingPDU_Indicator: GcTRUE,
                  timerStatusPeriodic: OMIT
                }
              }
            ],
            sS_dl_RLC_Mode:
            {
              dl_PayloadSize: 128,
              dl_RLCModeInfo:
              [
                ul_AM_RLC_Mode:
                {
                  transmissionRLC_Discard:
                  [
                    noDiscard: dat15
                  ],
                  transmissionWindowSize: tw32,
                  timerRST: tr500,
                  max_RST: rst1,
                  pollingInfo:
                  {
                    timerPollProhibit: tpp200,
                    timerPoll: tp200,
                    poll_PDU: OMIT,
                    poll_SDU: sdu1,
                    lastTransmissionPDU_Poll: GcTRUE,
                    lastRetransmissionPDU_Poll: GcTRUE,
                    pollWindow: pw99,
                    timerPollPeriodic: OMIT
                  }
                }
              ]
            }
          },
          rB_LogCH_Mapping:
          {
            uLlogicalChannelIdentity: 4,
            dLlogicalChannelIdentity: 4,
            logicalChannelType: OMIT,
            cn_DomainIdentity: OMIT
          }
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        rB_Identity: 0
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CMAC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        physicalChannelIdentity: 8
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CPHY_TrCH_Release_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        physicalChannelIdentity: 8
      ],
      trchConfigType:
      [
        nonDch: NULL
      ]
    }

TTCN PDU: CPHY_TrCH_Release_CNF

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        physicalChannelIdentity: 8
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        rB_Identity: -2
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CMAC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        physicalChannelIdentity: 5
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CPHY_TrCH_Release_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        physicalChannelIdentity: 5
      ],
      trchConfigType:
      [
        nonDch: NULL
      ]
    }

TTCN PDU: CPHY_TrCH_Release_CNF

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        physicalChannelIdentity: 5
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CMAC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        physicalChannelIdentity: 4
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CPHY_TrCH_Release_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        physicalChannelIdentity: 4
      ],
      trchConfigType:
      [
        nonDch: NULL
      ]
    }

TTCN PDU: CPHY_TrCH_Release_CNF

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      routingInfo:
      [
        physicalChannelIdentity: 4
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 1
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 2
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 3
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 4
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CMAC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        physicalChannelIdentity: 26
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CMAC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        physicalChannelIdentity: 20
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CPHY_TrCH_Release_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        physicalChannelIdentity: 26
      ],
      trchConfigType:
      [
        dch: normal
      ]
    }

TTCN PDU: CPHY_TrCH_Release_CNF

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        physicalChannelIdentity: 26
      ]
    }

TTCN PDU: CPHY_TrCH_Release_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        physicalChannelIdentity: 20
      ],
      trchConfigType:
      [
        dch: normal
      ]
    }

TTCN PDU: CPHY_TrCH_Release_CNF

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        physicalChannelIdentity: 20
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: 0
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CMAC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        physicalChannelIdentity: 8
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CPHY_TrCH_Release_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        physicalChannelIdentity: 8
      ],
      trchConfigType:
      [
        nonDch: NULL
      ]
    }

TTCN PDU: CPHY_TrCH_Release_CNF

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        physicalChannelIdentity: 8
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -2
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CMAC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        physicalChannelIdentity: 5
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CPHY_TrCH_Release_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        physicalChannelIdentity: 5
      ],
      trchConfigType:
      [
        nonDch: NULL
      ]
    }

TTCN PDU: CPHY_TrCH_Release_CNF

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        physicalChannelIdentity: 5
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CMAC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        physicalChannelIdentity: 4
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CPHY_TrCH_Release_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        physicalChannelIdentity: 4
      ],
      trchConfigType:
      [
        nonDch: NULL
      ]
    }

TTCN PDU: CPHY_TrCH_Release_CNF

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        physicalChannelIdentity: 4
      ]
    }