- No.: 2
- Timestamp: 12:20:43:680_0
- RFN: 134
- Chip: 0
- Event: Start Timer
- Source: tc_6_1_1_7 LINE 1
- Message Structure:
no details available
- Constraint:
t_Guard (300 Sec)
- BinaryMessage:

- No.: 128
- Timestamp: 12:20:43:698_0
- RFN: 135
- Chip: 28416
- Event: Send
- PCO: Ut
- Message: MMI_CmdReq
- Source: ts_MMI_UE_SwitchOff LINE 2
- Message Structure:
MMI_CmdReq
. (IA5StringType)cmd[-1] = "Please switch off the UE"
- Constraint:
ca_MMI_CmdReq
- BinaryMessage:
50 6c 65 61 73 65 20 73 77 69 74 63 68 20 6f 66 66 20 20 74 68 65 20 55 45

- No.: 132
- Timestamp: 12:20:45:728_0
- RFN: 338
- Chip: 28416
- Event: Receive
- PCO: Ut
- Message: MMI_CmdCnf
- Source: ts_MMI_UE_SwitchOff LINE 3
- Message Structure:
MMI_CmdCnf
. (BooleanType)result = TRUE
. (IA5StringType)resultString[0] = ""
- Constraint:
ca_MMI_CmdCnf
- BinaryMessage:
80

- No.: 137
- Timestamp: 12:20:45:729_2
- RFN: 338
- Chip: 31744
- Event: Send
- PCO: CPHY
- Message: CPHY_Ini_REQ
- Source: ts_SS_CellCfg:lt_CelllsAlreadyStarted LINE 5
- Message Structure:
CPHY_Ini_REQ
. (CPHY_Ini_REQ)CPHY_Ini_REQ[-1] = 0
- Constraint:
cas_InitReqDef
- BinaryMessage:
0a 01 00

- No.: 138
- Timestamp: 12:20:45:729_3
- RFN: 338
- Chip: 33024
- Event: Receive
- PCO: CPHY
- Message: CPHY_Ini_CNF
- Source: ts_SS_CellCfg:lt_CelllsAlreadyStarted LINE 6
- Message Structure:
CPHY_Ini_CNF
- Constraint:
car_IniCnf
- BinaryMessage:
30 02 05 00

- No.: 142
- Timestamp: 12:20:45:730_2
- RFN: 338
- Chip: 37376
- Event: Send
- PCO: CPHY
- Message: CPHY_Cell_Config_REQ
- Source: ts_SS_CellCfg LINE 6
- Message Structure:
CPHY_Cell_Config_REQ
. (IntegerType)cellId[-1] = 0
. (IntegerType)tcell[-1] = 0
. (IntegerType)sfnOffset[-1] = 0
. FrequencyInfo
. . modeSpecificInfo
. . . FrequencyInfoFDD
. . . . (IntegerType)uarfcn_UL[-1] = 9613
. . . . (IntegerType)uarfcn_DL[-1] = 10563
. (IntegerType)primaryScramblingCode_SS[-1] = 100
. CellTxPowerLevel
. (IntegerType)dLTxAttenuationLevel[-1] = 18
- Constraint:
ca_CellCfgReq
- BinaryMessage:
30 1d 02 01 00 02 01 00 02 01 00 30 0a 30 08 02 02 25 8d 02 02 29 43 02 01 64 05 00 02 01 12

- No.: 149
- Timestamp: 12:20:46:117_0
- RFN: 377
- Chip: 24064
- Event: Receive
- PCO: CPHY
- Message: CPHY_Cell_Config_CNF
- Source: ts_SS_CellCfg LINE 7
- Message Structure:
CPHY_Cell_Config_CNF
. (IntegerType)cellId[0] = 0
- Constraint:
ca_CellCfgCnf
- BinaryMessage:
30 03 02 01 00

- No.: 161
- Timestamp: 12:20:46:119_0
- RFN: 377
- Chip: 32000
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 3
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 0
. (RatType)ratType[0] = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . PrimaryCPICHInfo
. . . . (IntegerType)dl_TxPower_PCPICH[-1] = -60
. . . . (BooleanType)txdiversityIndicator = FALSE
- Constraint:
ca_pCPICH_Info
- BinaryMessage:
30 13 02 01 00 02 01 00 0a 01 00 30 08 30 06 02 01 c4 01 01 00

- No.: 165
- Timestamp: 12:20:46:124_0
- RFN: 378
- Chip: 13824
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 4
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 0
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 00

- No.: 166
- Timestamp: 12:20:46:125_0
- RFN: 378
- Chip: 16384
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 5
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 1
. (RatType)ratType[0] = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . PrimarySCHInfo
. . . . (BooleanType)tstdIndicator = FALSE
. . . . (IntegerType)dl_TxPower[-1] = -5
- Constraint:
ca_pSCH_Info
- BinaryMessage:
30 13 02 01 00 02 01 01 0a 01 00 30 08 30 06 01 01 00 02 01 fb

- No.: 170
- Timestamp: 12:20:46:128_0
- RFN: 378
- Chip: 29184
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 6
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 1
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 01

- No.: 171
- Timestamp: 12:20:46:129_0
- RFN: 378
- Chip: 31744
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 7
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 2
. (RatType)ratType[0] = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . SecondarySCHInfo
. . . . (BooleanType)tstdIndicator = FALSE
. . . . (IntegerType)dl_TxPower[-1] = -5
- Constraint:
ca_sSCH_Info
- BinaryMessage:
30 13 02 01 00 02 01 02 0a 01 00 30 08 30 06 01 01 00 02 01 fb

- No.: 175
- Timestamp: 12:20:46:267_0
- RFN: 392
- Chip: 25088
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 8
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 2
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 02

- No.: 176
- Timestamp: 12:20:46:268_0
- RFN: 392
- Chip: 27648
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 9
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 4
. (RatType)ratType[0] = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . PrimaryCCPCHInfo
. . . . (BooleanType)sttd_Indicator = FALSE
. . . . (IntegerType)dl_TxPower[-1] = -2
- Constraint:
ca_pCCPCH_Info
- BinaryMessage:
30 13 02 01 00 02 01 04 0a 01 00 30 08 30 06 01 01 00 02 01 fe

- No.: 180
- Timestamp: 12:20:46:275_0
- RFN: 393
- Chip: 16896
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 10
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 4
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 04

- No.: 181
- Timestamp: 12:20:46:277_0
- RFN: 393
- Chip: 24832
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Config_REQ
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 11
- Message Structure:
CPHY_TrCH_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 4
. (RatType)ratType[0] = 0
. TrChConfigType
. CphyTrchConfigReq
. . SS_ActivationTime
. . ulconnectedTrCHList
. . TFCS
. . dlconnectedTrCHList
. . . CphyTrchConfigReq_setseq_1
. . . . (IntegerType)trchid[-1] = 11
. . . . (SS_DL_TransportChannelType)dl_TransportChannelType[0] = 2
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size[-1] = 246
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional[0] = 0
. . . . . . (IntegerType)rateMatchingAttribute[-1] = 1
. . . . . . (CRC_Size)crc_Size[0] = 3
. . TFCS
. . . ExplicitTFCS_Configuration
. . . . TFCS_ReconfAdd
. . . . . ctfcSize
. . . . . . ctfc2Bit
. . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . (IntegerType)ctfc2[-1] = 0
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . fdd
. . . . . . . . . . . . . (IntegerType)gainFactorBetaC[-1] = 11
. . . . . . . . . . . (IntegerType)gainFactorBetaD[-1] = 15
. . . . . . . . . . . (IntegerType)referenceTFC_ID[-1] = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
- Constraint:
ca_BCH_InfoActNow
- BinaryMessage:
30 4c 02 01 00 02 01 04 0a 01 00 05 00 30 3f 05 00 30 23 30 21 02 01 0b 0a 01 02 30 19 30 0c 30 0a 02 02 00 f6 30 02 05 00 05 00 30 09 0a 01 00 02 01 01 0a 01 03 30 16 30 14 30 12 02 01 00 30 0d 30 0b 30 03 02 01 0b 02 01 0f 02 01 00

- No.: 185
- Timestamp: 12:20:46:284_0
- RFN: 394
- Chip: 13056
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Config_CNF
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 12
- Message Structure:
CPHY_TrCH_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 4
- Constraint:
ca_TrChCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 04

- No.: 186
- Timestamp: 12:20:46:287_0
- RFN: 394
- Chip: 25088
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 13
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 4
. (RatType)ratType[0] = 0
. configMessage
. . CmacConfigReq
. . . SS_ActivationTime
. . . UE_Info
. . . . U_RNTI
. . . . (BitStringType)c_RNTI[16] = -
. . . TrCHInfo
. . . . ulconnectedTrCHList
. . . . TFCS
. . . . dlconnectedTrCHList
. . . . . TrCHInfo_setseq_1
. . . . . . (IntegerType)trchid[-1] = 11
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size[-1] = 246
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional[0] = 0
. . . . . . . . (IntegerType)rateMatchingAttribute[-1] = 1
. . . . . . . . (CRC_Size)crc_Size[0] = 3
. . . . TFCS
. . . . . ExplicitTFCS_Configuration
. . . . . . TFCS_ReconfAdd
. . . . . . . ctfcSize
. . . . . . . . ctfc2Bit
. . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . (IntegerType)ctfc2[-1] = 0
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC[-1] = 11
. . . . . . . . . . . . . (IntegerType)gainFactorBetaD[-1] = 15
. . . . . . . . . . . . . (IntegerType)referenceTFC_ID[-1] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . TrCH_LogCHMappingList1
. . . . ulconnectedTrCHList
. . . . dlconnectedTrCHList
. . . . . TrCH_LogCHMappingList1_setseq_1
. . . . . . (IntegerType)trchid[-1] = 11
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation[0] = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType[0] = 2
. . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . . . (LogicalChannelType)logicalChannelType[0] = 0
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 1
. . . . . . . . (IntegerType)rB_Identity[-1] = -1
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_CMAC_CfgInfo
- BinaryMessage:
30 6e 02 01 00 02 01 04 0a 01 00 30 63 05 00 30 00 30 3a 30 20 30 1e 02 01 0b 30 19 30 0c 30 0a 02 02 00 f6 30 02 05 00 05 00 30 09 0a 01 00 02 01 01 0a 01 03 30 16 30 14 30 12 02 01 00 30 0d 30 0b 30 03 02 01 0b 02 01 0f 02 01 00 30 21 30 1f 30 1d 02 01 0b 30 18 30 16 30 11 0a 01 00 0a 01 02 02 01 01 0a 01 00 05 00 02 01 01 02 01 ff

- No.: 190
- Timestamp: 12:20:46:290_0
- RFN: 394
- Chip: 36864
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 14
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 4
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 04

- No.: 226
- Timestamp: 12:20:46:295_1
- RFN: 395
- Chip: 17152
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_PCH_2FACH_CCCH_DCCH_BCCH_DTCH_Cfg LINE 3
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 5
. (RatType)ratType[0] = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . SecondaryCCPCHInfo
. . . . (IntegerType)scramblingCode[-1] = 0
. . . . SF256_AndCodeNumber
. . . . . (IntegerType)sf64[-1] = 1
. . . . (IntegerType)sCCPCHSlotFormat[-1] = 8
. . . . (IntegerType)timingOffset[-1] = 0
. . . . (PositionFixedOrFlexible)positionFixedOrFlexible[0] = 1
. . . . (BooleanType)sttd_Indicator = FALSE
. . . . (IntegerType)dl_TxPower[-1] = -2
. . . . (IntegerType)powerOffsetOfTFCI_PO1[-1] = 6
. . . . (IntegerType)powerOffsetOfPILOT_PO3[-1] = 6
- Constraint:
ca_sCCPCH_Info
- BinaryMessage:
30 28 02 01 00 02 01 05 0a 01 00 30 1d 30 1b 02 01 00 02 01 01 02 01 08 02 01 00 0a 01 01 01 01 00 02 01 fe 02 01 06 02 01 06

- No.: 230
- Timestamp: 12:20:46:301_0
- RFN: 395
- Chip: 37376
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_PCH_2FACH_CCCH_DCCH_BCCH_DTCH_Cfg LINE 4
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 5
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 05

- No.: 231
- Timestamp: 12:20:46:306_0
- RFN: 396
- Chip: 20224
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Config_REQ
- Source: ts_SS_PCH_2FACH_CCCH_DCCH_BCCH_DTCH_Cfg LINE 5
- Message Structure:
CPHY_TrCH_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 5
. (RatType)ratType[0] = 0
. TrChConfigType
. CphyTrchConfigReq
. . SS_ActivationTime
. . ulconnectedTrCHList
. . TFCS
. . dlconnectedTrCHList
. . . CphyTrchConfigReq_setseq_1
. . . . (IntegerType)trchid[-1] = 12
. . . . (SS_DL_TransportChannelType)dl_TransportChannelType[0] = 3
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size[-1] = 240
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional[0] = 0
. . . . . . (IntegerType)rateMatchingAttribute[-1] = 230
. . . . . . (CRC_Size)crc_Size[0] = 3
. . . CphyTrchConfigReq_setseq_1
. . . . (IntegerType)trchid[-1] = 13
. . . . (SS_DL_TransportChannelType)dl_TransportChannelType[0] = 1
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size[-1] = 168
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . (IntegerType)small[-1] = 2
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional[0] = 0
. . . . . . (IntegerType)rateMatchingAttribute[-1] = 220
. . . . . . (CRC_Size)crc_Size[0] = 3
. . . CphyTrchConfigReq_setseq_1
. . . . (IntegerType)trchid[-1] = 14
. . . . (SS_DL_TransportChannelType)dl_TransportChannelType[0] = 1
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size[-1] = 360
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . (IntegerType)rateMatchingAttribute[-1] = 130
. . . . . . (CRC_Size)crc_Size[0] = 3
. . TFCS
. . . ExplicitTFCS_Configuration
. . . . TFCS_ReconfAdd
. . . . . ctfcSize
. . . . . . ctfc4Bit
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4[-1] = 0
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4[-1] = 1
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4[-1] = 2
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4[-1] = 3
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4[-1] = 4
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4[-1] = 5
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4[-1] = 6
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4[-1] = 8
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . fdd
. . . . . . . . . . . . . (IntegerType)gainFactorBetaC[-1] = 11
. . . . . . . . . . . (IntegerType)gainFactorBetaD[-1] = 15
. . . . . . . . . . . (IntegerType)referenceTFC_ID[-1] = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
- Constraint:
ca_PCH_2_FACH_InfoActNow
- BinaryMessage:
30 81 e4 02 01 00 02 01 05 0a 01 00 05 00 30 81 d6 05 00 30 74 30 24 02 01 0c 0a 01 03 30 1c 30 0e 30 0c 02 02 00 f0 30 04 05 00 05 00 05 00 30 0a 0a 01 00 02 02 00 e6 0a 01 03 30 27 02 01 0d 0a 01 01 30 1f 30 11 30 0f 02 02 00 a8 30 07 05 00 05 00 02 01 02 05 00 30 0a 0a 01 00 02 02 00 dc 0a 01 03 30 23 02 01 0e 0a 01 01 30 1b 30 0e 30 0c 02 02 01 68 30 04 05 00 05 00 05 00 30 09 05 00 02 02 00 82 0a 01 03 30 5c 30 5a 30 08 02 01 00 30 03 02 01 00 30 08 02 01 01 30 03 02 01 00 30 08 02 01 02 30 03 02 01 00 30 08 02 01 03 30 03 02 01 00 30 08 02 01 04 30 03 02 01 00 30 08 02 01 05 30 03 02 01 00 30 08 02 01 06 30 03 02 01 00 30 12 02 01 08 30 0d 30 0b 30 03 02 01 0b 02 01 0f 02 01 00

- No.: 235
- Timestamp: 12:20:46:315_0
- RFN: 397
- Chip: 15360
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Config_CNF
- Source: ts_SS_PCH_2FACH_CCCH_DCCH_BCCH_DTCH_Cfg LINE 6
- Message Structure:
CPHY_TrCH_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 5
- Constraint:
ca_TrChCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 05

- No.: 236
- Timestamp: 12:20:46:327_0
- RFN: 398
- Chip: 23552
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_SS_PCH_2FACH_CCCH_DCCH_BCCH_DTCH_Cfg LINE 7
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 5
. (RatType)ratType[0] = 0
. configMessage
. . CmacConfigReq
. . . SS_ActivationTime
. . . UE_Info
. . . . U_RNTI
. . . . . (BitStringType)srnc_Identity[12] = "000000000001"
. . . . . (BitStringType)s_RNTI[20] = "00000000000000000001"
. . . . (BitStringType)c_RNTI[16] = "0000000000000001"
. . . TrCHInfo
. . . . ulconnectedTrCHList
. . . . TFCS
. . . . dlconnectedTrCHList
. . . . . TrCHInfo_setseq_1
. . . . . . (IntegerType)trchid[-1] = 12
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size[-1] = 240
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional[0] = 0
. . . . . . . . (IntegerType)rateMatchingAttribute[-1] = 230
. . . . . . . . (CRC_Size)crc_Size[0] = 3
. . . . . TrCHInfo_setseq_1
. . . . . . (IntegerType)trchid[-1] = 13
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size[-1] = 168
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . (IntegerType)small[-1] = 2
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional[0] = 0
. . . . . . . . (IntegerType)rateMatchingAttribute[-1] = 220
. . . . . . . . (CRC_Size)crc_Size[0] = 3
. . . . . TrCHInfo_setseq_1
. . . . . . (IntegerType)trchid[-1] = 14
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size[-1] = 360
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . (IntegerType)rateMatchingAttribute[-1] = 130
. . . . . . . . (CRC_Size)crc_Size[0] = 3
. . . . TFCS
. . . . . ExplicitTFCS_Configuration
. . . . . . TFCS_ReconfAdd
. . . . . . . ctfcSize
. . . . . . . . ctfc4Bit
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4[-1] = 0
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4[-1] = 1
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4[-1] = 2
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4[-1] = 3
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4[-1] = 4
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4[-1] = 5
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4[-1] = 6
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4[-1] = 8
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC[-1] = 11
. . . . . . . . . . . . . (IntegerType)gainFactorBetaD[-1] = 15
. . . . . . . . . . . . . (IntegerType)referenceTFC_ID[-1] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . TrCH_LogCHMappingList1
. . . . ulconnectedTrCHList
. . . . dlconnectedTrCHList
. . . . . TrCH_LogCHMappingList1_setseq_1
. . . . . . (IntegerType)trchid[-1] = 12
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation[0] = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType[0] = 3
. . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . . . (LogicalChannelType)logicalChannelType[0] = 1
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 1
. . . . . . . . (IntegerType)rB_Identity[-1] = -2
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
. . . . . TrCH_LogCHMappingList1_setseq_1
. . . . . . (IntegerType)trchid[-1] = 13
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation[0] = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType[0] = 1
. . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 6
. . . . . . . . . . (LogicalChannelType)logicalChannelType[0] = 0
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 6
. . . . . . . . (IntegerType)rB_Identity[-1] = -3
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation[0] = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType[0] = 1
. . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 5
. . . . . . . . . . (LogicalChannelType)logicalChannelType[0] = 2
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 1
. . . . . . . . (IntegerType)rB_Identity[-1] = 0
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation[0] = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType[0] = 1
. . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . . . (LogicalChannelType)logicalChannelType[0] = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 1
. . . . . . . . (IntegerType)rB_Identity[-1] = 1
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation[0] = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType[0] = 1
. . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 2
. . . . . . . . . . (LogicalChannelType)logicalChannelType[0] = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 2
. . . . . . . . (IntegerType)rB_Identity[-1] = 2
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation[0] = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType[0] = 1
. . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 3
. . . . . . . . . . (LogicalChannelType)logicalChannelType[0] = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 3
. . . . . . . . (IntegerType)rB_Identity[-1] = 3
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation[0] = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType[0] = 1
. . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 4
. . . . . . . . . . (LogicalChannelType)logicalChannelType[0] = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 4
. . . . . . . . (IntegerType)rB_Identity[-1] = 4
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
. . . . . TrCH_LogCHMappingList1_setseq_1
. . . . . . (IntegerType)trchid[-1] = 14
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation[0] = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType[0] = 1
. . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 7
. . . . . . . . . . (LogicalChannelType)logicalChannelType[0] = 5
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 8
. . . . . . . . (IntegerType)rB_Identity[-1] = 20
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_CMAC_CfgInfo
- BinaryMessage:
30 82 01 ce 02 01 00 02 01 05 0a 01 00 30 82 01 c1 05 00 30 12 30 0b 03 03 04 00 00 03 04 04 00 00 00 03 03 00 00 00 30 81 cb 30 6b 30 21 02 01 0c 30 1c 30 0e 30 0c 02 02 00 f0 30 04 05 00 05 00 05 00 30 0a 0a 01 00 02 02 00 e6 0a 01 03 30 24 02 01 0d 30 1f 30 11 30 0f 02 02 00 a8 30 07 05 00 05 00 02 01 02 05 00 30 0a 0a 01 00 02 02 00 dc 0a 01 03 30 20 02 01 0e 30 1b 30 0e 30 0c 02 02 01 68 30 04 05 00 05 00 05 00 30 09 05 00 02 02 00 82 0a 01 03 30 5c 30 5a 30 08 02 01 00 30 03 02 01 00 30 08 02 01 01 30 03 02 01 00 30 08 02 01 02 30 03 02 01 00 30 08 02 01 03 30 03 02 01 00 30 08 02 01 04 30 03 02 01 00 30 08 02 01 05 30 03 02 01 00 30 08 02 01 06 30 03 02 01 00 30 12 02 01 08 30 0d 30 0b 30 03 02 01 0b 02 01 0f 02 01 00 30 81 da 30 81 d7 30 1d 02 01 0c 30 18 30 16 30 11 0a 01 00 0a 01 03 02 01 01 0a 01 01 05 00 02 01 01 02 01 fe 30 81 96 02 01 0d 30 81 90 30 16 30 11 0a 01 00 0a 01 01 02 01 06 0a 01 00 05 00 02 01 06 02 01 fd 30 16 30 11 0a 01 00 0a 01 01 02 01 05 0a 01 02 05 00 02 01 01 02 01 00 30 16 30 11 0a 01 00 0a 01 01 02 01 01 0a 01 04 05 00 02 01 01 02 01 01 30 16 30 11 0a 01 00 0a 01 01 02 01 02 0a 01 04 05 00 02 01 02 02 01 02 30 16 30 11 0a 01 00 0a 01 01 02 01 03 0a 01 04 05 00 02 01 03 02 01 03 30 16 30 11 0a 01 00 0a 01 01 02 01 04 0a 01 04 05 00 02 01 04 02 01 04 30 1d 02 01 0e 30 18 30 16 30 11 0a 01 00 0a 01 01 02 01 07 0a 01 05 05 00 02 01 08 02 01 14

- No.: 240
- Timestamp: 12:20:46:349_0
- RFN: 400
- Chip: 33024
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_SS_PCH_2FACH_CCCH_DCCH_BCCH_DTCH_Cfg LINE 8
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 5
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 05

- No.: 241
- Timestamp: 12:20:46:350_0
- RFN: 400
- Chip: 36352
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_PCH_2FACH_CCCH_DCCH_BCCH_DTCH_Cfg LINE 9
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 6
. (RatType)ratType[0] = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . PICHInfo
. . . . PICH_Info
. . . . . fdd
. . . . . . (IntegerType)channelisationCode256[-1] = 2
. . . . . . (PI_CountPerFrame)pi_CountPerFrame[0] = 0
. . . . . . (BooleanType)sttd_Indicator = FALSE
. . . . (IntegerType)dl_TxPower[-1] = -5
. . . . (IntegerType)sccpchId_associated[-1] = 5
- Constraint:
ca_PICH_Info
- BinaryMessage:
30 1e 02 01 00 02 01 06 0a 01 00 30 13 30 11 30 09 02 01 02 0a 01 00 01 01 00 02 01 fb 02 01 05

- No.: 245
- Timestamp: 12:20:46:356_0
- RFN: 401
- Chip: 21504
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_PCH_2FACH_CCCH_DCCH_BCCH_DTCH_Cfg LINE 10
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 6
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 06

- No.: 253
- Timestamp: 12:20:46:358_0
- RFN: 401
- Chip: 27392
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_RACH_CCCH_DCCH_DTCH_Cfg LINE 3
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 7
. (RatType)ratType[0] = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . AICHInfo
. . . . AICH_Info
. . . . . (IntegerType)channelisationCode256[-1] = 3
. . . . . (BooleanType)sttd_Indicator = FALSE
. . . . . (AICH_TransmissionTiming)aich_TransmissionTiming[0] = 0
. . . . (IntegerType)dl_TxPower[-1] = -5
- Constraint:
ca_AichInfo
- BinaryMessage:
30 1b 02 01 00 02 01 07 0a 01 00 30 10 30 0e 30 09 02 01 03 01 01 00 0a 01 00 02 01 fb

- No.: 257
- Timestamp: 12:20:46:365_0
- RFN: 402
- Chip: 15616
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_RACH_CCCH_DCCH_DTCH_Cfg LINE 4
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 7
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 07

- No.: 258
- Timestamp: 12:20:46:366_0
- RFN: 402
- Chip: 18944
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_RACH_CCCH_DCCH_DTCH_Cfg LINE 5
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 8
. (RatType)ratType[0] = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . PRACHInfo
. . . . fdd_tdd
. . . . . fdd
. . . . . . (BitStringType)preambleSignature[16] = "0000000011111111"
. . . . . . (SF_PRACH)spreadingFactorForDataPart[0] = 1
. . . . . . (IntegerType)preambleScramblingCode[-1] = 0
. . . . . . (PuncturingLimit)puncturingLimit[0] = 15
. . . . . . (BitStringType)accessSlot[12] = "111111111111"
- Constraint:
ca_PRACH_Info
- BinaryMessage:
30 22 02 01 00 02 01 08 0a 01 00 30 17 30 15 30 13 03 03 00 00 00 0a 01 01 02 01 00 0a 01 0f 03 03 04 ff ff

- No.: 262
- Timestamp: 12:20:46:369_0
- RFN: 402
- Chip: 33792
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_RACH_CCCH_DCCH_DTCH_Cfg LINE 6
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 8
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 00 02 01 08

- No.: 263
- Timestamp: 12:20:46:371_0
- RFN: 403
- Chip: 3328
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Config_REQ
- Source: ts_SS_RACH_CCCH_DCCH_DTCH_Cfg LINE 7
- Message Structure:
CPHY_TrCH_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 8
. (RatType)ratType[0] = 0
. TrChConfigType
. CphyTrchConfigReq
. . SS_ActivationTime
. . ulconnectedTrCHList
. . . CphyTrchConfigReq_setseq_0
. . . . (IntegerType)trchid[-1] = 15
. . . . (SS_UL_TransportChannelType)ul_TransportChannelType[0] = 1
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size[-1] = 168
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size[-1] = 360
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional[0] = 0
. . . . . . (IntegerType)rateMatchingAttribute[-1] = 150
. . . . . . (CRC_Size)crc_Size[0] = 3
. . TFCS
. . . ExplicitTFCS_Configuration
. . . . TFCS_ReconfAdd
. . . . . ctfcSize
. . . . . . ctfc2Bit
. . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . (IntegerType)ctfc2[-1] = 0
. . . . . . . . PowerOffsetInformation
. . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . (IntegerType)ctfc2[-1] = 1
. . . . . . . . PowerOffsetInformation
. . dlconnectedTrCHList
. . TFCS
- Constraint:
cab_RACH_InfoActNow
- BinaryMessage:
30 4f 02 01 00 02 01 08 0a 01 00 05 00 30 42 05 00 30 30 30 2e 02 01 0f 0a 01 01 30 26 30 18 30 0a 02 02 00 a8 30 02 05 00 05 00 30 0a 02 02 01 68 30 02 05 00 05 00 30 0a 0a 01 00 02 02 00 96 0a 01 03 30 0c 30 0a 30 03 02 01 00 30 03 02 01 01

- No.: 267
- Timestamp: 12:20:46:381_0
- RFN: 404
- Chip: 1024
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Config_CNF
- Source: ts_SS_RACH_CCCH_DCCH_DTCH_Cfg LINE 8
- Message Structure:
CPHY_TrCH_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 8
- Constraint:
ca_TrChCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 08

- No.: 268
- Timestamp: 12:20:46:386_0
- RFN: 404
- Chip: 22528
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_SS_RACH_CCCH_DCCH_DTCH_Cfg LINE 9
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 8
. (RatType)ratType[0] = 0
. configMessage
. . CmacConfigReq
. . . SS_ActivationTime
. . . UE_Info
. . . . U_RNTI
. . . . (BitStringType)c_RNTI[16] = "0000000000000001"
. . . TrCHInfo
. . . . ulconnectedTrCHList
. . . . . TrCHInfo_setseq_0
. . . . . . (IntegerType)trchid[-1] = 15
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size[-1] = 168
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size[-1] = 360
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional[0] = 0
. . . . . . . . (IntegerType)rateMatchingAttribute[-1] = 150
. . . . . . . . (CRC_Size)crc_Size[0] = 3
. . . . TFCS
. . . . . ExplicitTFCS_Configuration
. . . . . . TFCS_ReconfAdd
. . . . . . . ctfcSize
. . . . . . . . ctfc2Bit
. . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . (IntegerType)ctfc2[-1] = 0
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . (IntegerType)ctfc2[-1] = 1
. . . . . . . . . . PowerOffsetInformation
. . . . dlconnectedTrCHList
. . . . TFCS
. . . TrCH_LogCHMappingList1
. . . . ulconnectedTrCHList
. . . . . TrCH_LogCHMappingList1_setseq_0
. . . . . . (IntegerType)trchid[-1] = 15
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation[0] = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType[0] = 1
. . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 5
. . . . . . . . . . (LogicalChannelType)logicalChannelType[0] = 2
. . . . . . . . (IntegerType)rB_Identity[-1] = 0
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation[0] = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType[0] = 1
. . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . . . (LogicalChannelType)logicalChannelType[0] = 4
. . . . . . . . (IntegerType)rB_Identity[-1] = 1
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation[0] = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType[0] = 1
. . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 2
. . . . . . . . . . (LogicalChannelType)logicalChannelType[0] = 4
. . . . . . . . (IntegerType)rB_Identity[-1] = 2
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation[0] = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType[0] = 1
. . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 3
. . . . . . . . . . (LogicalChannelType)logicalChannelType[0] = 4
. . . . . . . . (IntegerType)rB_Identity[-1] = 3
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation[0] = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType[0] = 1
. . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 4
. . . . . . . . . . (LogicalChannelType)logicalChannelType[0] = 4
. . . . . . . . (IntegerType)rB_Identity[-1] = 4
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation[0] = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType[0] = 1
. . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 7
. . . . . . . . . . (LogicalChannelType)logicalChannelType[0] = 5
. . . . . . . . (IntegerType)rB_Identity[-1] = 20
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
. . . . dlconnectedTrCHList
- Constraint:
ca_CMAC_CfgInfo
- BinaryMessage:
30 81 d1 02 01 00 02 01 08 0a 01 00 30 81 c5 05 00 30 05 03 03 00 00 00 30 3d 30 2d 30 2b 02 01 0f 30 26 30 18 30 0a 02 02 00 a8 30 02 05 00 05 00 30 0a 02 02 01 68 30 02 05 00 05 00 30 0a 0a 01 00 02 02 00 96 0a 01 03 30 0c 30 0a 30 03 02 01 00 30 03 02 01 01 30 7b 30 79 30 77 02 01 0f 30 72 30 11 30 0c 0a 01 00 0a 01 01 02 01 05 0a 01 02 02 01 00 30 11 30 0c 0a 01 00 0a 01 01 02 01 01 0a 01 04 02 01 01 30 11 30 0c 0a 01 00 0a 01 01 02 01 02 0a 01 04 02 01 02 30 11 30 0c 0a 01 00 0a 01 01 02 01 03 0a 01 04 02 01 03 30 11 30 0c 0a 01 00 0a 01 01 02 01 04 0a 01 04 02 01 04 30 11 30 0c 0a 01 00 0a 01 01 02 01 07 0a 01 05 02 01 14

- No.: 272
- Timestamp: 12:20:46:405_0
- RFN: 406
- Chip: 19200
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_SS_RACH_CCCH_DCCH_DTCH_Cfg LINE 10
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 8
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 08

- No.: 275
- Timestamp: 12:20:46:407_0
- RFN: 406
- Chip: 24320
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB_BCCH_BCH_Cfg LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 246
. . . . . UL_RLC_Mode
. . . . . . UL_TM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . (BooleanType)segmentationIndication = FALSE
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[0] = -
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 1
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_BCCH_Info
- BinaryMessage:
30 1d 02 01 00 02 01 ff 0a 01 00 30 12 30 0b 30 09 02 02 00 f6 30 03 01 01 00 30 03 02 01 01

- No.: 279
- Timestamp: 12:20:46:409_0
- RFN: 406
- Chip: 32256
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB_BCCH_BCH_Cfg LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 282
- Timestamp: 12:20:46:410_0
- RFN: 406
- Chip: 36096
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB_PCCH_Cfg LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -2
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 240
. . . . . UL_RLC_Mode
. . . . . . UL_TM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . (BooleanType)segmentationIndication = FALSE
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[0] = -
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 1
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_PCCH_Info
- BinaryMessage:
30 1d 02 01 00 02 01 fe 0a 01 00 30 12 30 0b 30 09 02 02 00 f0 30 03 01 01 00 30 03 02 01 01

- No.: 286
- Timestamp: 12:20:46:415_0
- RFN: 407
- Chip: 18432
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB_PCCH_Cfg LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 fe

- No.: 289
- Timestamp: 12:20:46:416_1
- RFN: 407
- Chip: 23296
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB0_Cfg LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 0
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 152
. . . . . UL_RLC_Mode
. . . . . . UL_UM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (NoExplicitDiscard)timerBasedNoExplicit[0] = 9
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[0] = -
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 5
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_UM_DL_Info
- BinaryMessage:
30 1d 02 01 00 02 01 00 0a 01 00 30 12 30 0b 30 09 02 02 00 98 30 03 0a 01 09 30 03 02 01 05

- No.: 293
- Timestamp: 12:20:46:419_0
- RFN: 407
- Chip: 31744
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB0_Cfg LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 0
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 00

- No.: 294
- Timestamp: 12:20:46:420_0
- RFN: 407
- Chip: 35840
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB0_Cfg LINE 3
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 0
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_TM_RLC_Mode
. . . . . . (BooleanType)segmentationIndication = FALSE
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 166
. . . . . UL_RLC_Mode
. . . . . . UL_TM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . (BooleanType)segmentationIndication = FALSE
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 5
. . . . (IntegerType)dLlogicalChannelIdentity[0] = -
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_TM_UL_Info
- BinaryMessage:
30 22 02 01 00 02 01 00 0a 01 00 30 17 30 10 30 03 01 01 00 30 09 02 02 00 a6 30 03 01 01 00 30 03 02 01 05

- No.: 298
- Timestamp: 12:20:46:427_0
- RFN: 408
- Chip: 24576
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB0_Cfg LINE 4
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 0
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 00

- No.: 301
- Timestamp: 12:20:46:428_0
- RFN: 408
- Chip: 29952
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 1
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 136
. . . . . UL_RLC_Mode
. . . . . . UL_UM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (NoExplicitDiscard)timerBasedNoExplicit[0] = 9
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 1
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 1
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_UM_Info
- BinaryMessage:
30 22 02 01 ff 02 01 01 0a 01 00 30 17 30 0d 05 00 30 09 02 02 00 88 30 03 0a 01 09 30 06 02 01 01 02 01 01

- No.: 305
- Timestamp: 12:20:46:436_0
- RFN: 409
- Chip: 19968
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 306
- Timestamp: 12:20:46:437_0
- RFN: 409
- Chip: 25856
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 3
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 2
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 2
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 2
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 02 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 13 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 02 02 01 02

- No.: 310
- Timestamp: 12:20:46:450_0
- RFN: 410
- Chip: 36864
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 4
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 311
- Timestamp: 12:20:46:451_0
- RFN: 411
- Chip: 4352
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 5
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 3
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 3
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 3
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 03 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 13 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 03 02 01 03

- No.: 315
- Timestamp: 12:20:46:465_0
- RFN: 412
- Chip: 19712
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 6
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 3
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 316
- Timestamp: 12:20:46:467_0
- RFN: 412
- Chip: 25856
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 7
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 4
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 4
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 4
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 04 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 13 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 04 02 01 04

- No.: 320
- Timestamp: 12:20:46:481_0
- RFN: 414
- Chip: 2304
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 8
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 4
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 323
- Timestamp: 12:20:46:482_0
- RFN: 414
- Chip: 6656
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB_BCCH_FACH_Cfg LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -3
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 166
. . . . . UL_RLC_Mode
. . . . . . UL_TM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . (BooleanType)segmentationIndication = TRUE
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[0] = -
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 6
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_TM_DL_Info
- BinaryMessage:
30 1d 02 01 00 02 01 fd 0a 01 00 30 12 30 0b 30 09 02 02 00 a6 30 03 01 01 ff 30 03 02 01 06

- No.: 327
- Timestamp: 12:20:46:486_0
- RFN: 414
- Chip: 20992
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB_BCCH_FACH_Cfg LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -3
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 fd

- No.: 330
- Timestamp: 12:20:46:487_0
- RFN: 414
- Chip: 27904
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB20_AM_PS_Cfg LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 20
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 5
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 320
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 5
. . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . (MaxRST)max_RST[0] = 1
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 7
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 7
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_AM_Info_RAB
- BinaryMessage:
30 4d 02 01 ff 02 01 14 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 05 30 06 0a 01 13 01 01 ff 30 26 02 02 01 40 30 20 0a 01 0a 0a 01 05 0a 01 09 0a 01 01 30 12 0a 01 13 0a 01 13 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 07 02 01 07

- No.: 334
- Timestamp: 12:20:46:505_0
- RFN: 416
- Chip: 17152
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB20_AM_PS_Cfg LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 20
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 14

- No.: 396
- Timestamp: 12:20:46:520_0
- RFN: 417
- Chip: 36864
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 10
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 0a

- No.: 401
- Timestamp: 12:20:46:525_0
- RFN: 418
- Chip: 19712
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB1_LongNeighCellInfo LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 402
- Timestamp: 12:20:46:526_0
- RFN: 418
- Chip: 23552
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB1_LongNeighCellInfo LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 1
. . . . . . . (BitStringType)sib_Data_variable[-1] = "1100010000000000000001011000100000001000000000100001000111100000000101111111111111111111111110100101100011011011100110111111111010010101011101010011101001110111111001111010011"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 2
. . . . . . . (BitStringType)sib_Data_variable[-1] = "00000000000000000001"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 24 02 01 00 02 01 ff 00 0e 21 ae c4 00 05 88 08 02 11 e0 17 ff ff fa 58 db 9b fe 95 75 3a 77 e7 a6 21 30 00 01

- No.: 414
- Timestamp: 12:20:46:529_4
- RFN: 418
- Chip: 36096
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 10
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 0a

- No.: 419
- Timestamp: 12:20:46:546_0
- RFN: 420
- Chip: 19456
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB2_LongNeighCellInfo LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 420
- Timestamp: 12:20:46:547_0
- RFN: 420
- Chip: 22784
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB2_LongNeighCellInfo LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 1
. . . . . . . (BitStringType)sib_Data_variable[-1] = "1100010000000000000001011000100000001000000000100001000111100000000101111111111111111111111110100101100011011011100110111111111010010101011101010011101001110111111001111010011"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 2
. . . . . . . (BitStringType)sib_Data_variable[-1] = "00000000000000000001"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 24 02 01 00 02 01 ff 00 0e 21 ae c4 00 05 88 08 02 11 e0 17 ff ff fa 58 db 9b fe 95 75 3a 77 e7 a6 21 30 00 01

- No.: 432
- Timestamp: 12:20:46:550_2
- RFN: 420
- Chip: 35328
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 7
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 07

- No.: 437
- Timestamp: 12:20:46:566_0
- RFN: 422
- Chip: 19968
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB3_LongNeighCellInfo LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 438
- Timestamp: 12:20:46:567_0
- RFN: 422
- Chip: 23040
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB3_LongNeighCellInfo LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 7
. . . . . . . (BitStringType)sib_Data_variable[-1] = "100000101000000010000001"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 3
. . . . . . . (BitStringType)sib_Data_variable[-1] = "010000000000000000000000000000001011001100011000010000000000001000000100011111111111111111111111"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 1b 02 01 00 02 01 ff 00 0e 27 17 82 80 81 1a fa 00 00 00 05 98 c2 00 10 23 ff ff f8

- No.: 450
- Timestamp: 12:20:46:570_1
- RFN: 422
- Chip: 35328
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 31
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 1f

- No.: 455
- Timestamp: 12:20:46:576_0
- RFN: 423
- Chip: 20480
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB4_LongNeighCellInfo LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 456
- Timestamp: 12:20:46:577_0
- RFN: 423
- Chip: 23552
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB4_LongNeighCellInfo LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 7
. . . . . . . (BitStringType)sib_Data_variable[-1] = "100000101000000010000001"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 4
. . . . . . . (BitStringType)sib_Data_variable[-1] = "0000000000000000000000000000000101100110001100001000000000000100000010001110111"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 19 02 01 00 02 01 ff 00 0e 27 17 82 80 81 22 70 00 00 00 0b 31 84 00 20 47 70

- No.: 473
- Timestamp: 12:20:46:585_0
- RFN: 424
- Chip: 15616
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 22
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 16

- No.: 478
- Timestamp: 12:20:46:587_0
- RFN: 424
- Chip: 23808
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB5_LongNeighCellInfo LINE 41
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 479
- Timestamp: 12:20:46:588_0
- RFN: 424
- Chip: 26112
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB5_LongNeighCellInfo LINE 42
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 08 02 01 00 02 01 ff 00 00

- No.: 483
- Timestamp: 12:20:46:589_0
- RFN: 424
- Chip: 29696
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 18
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 12

- No.: 488
- Timestamp: 12:20:46:596_0
- RFN: 425
- Chip: 20480
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB5_LongNeighCellInfo LINE 44
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 489
- Timestamp: 12:20:46:597_0
- RFN: 425
- Chip: 23552
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB5_LongNeighCellInfo LINE 45
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . FirstSegment
. . . . . . (SIB_Type)sib_Type[0] = 5
. . . . . . (IntegerType)seg_Count[-1] = 3
. . . . . . (BitStringType)sib_Data_fixed[222] = "000101010100010000111110000000001111111101000011111111111111110111010010000100001111000000101001000011000000101010100101010110000000000000001100110001011011010101111110001010111010000011111110100000111111101000001111111010"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 25 02 01 00 02 01 ff 00 02 52 15 44 3e 00 ff 43 ff fd d2 10 f0 29 0c 0a a5 58 00 0c c5 b5 7e 2b a0 fe 83 fa 0f e8

- No.: 493
- Timestamp: 12:20:46:598_1
- RFN: 425
- Chip: 27904
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 19
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 13

- No.: 498
- Timestamp: 12:20:46:606_0
- RFN: 426
- Chip: 19200
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB5_LongNeighCellInfo LINE 47
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 499
- Timestamp: 12:20:46:606_1
- RFN: 426
- Chip: 22272
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB5_LongNeighCellInfo LINE 48
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . SubsequentSegment
. . . . . . (SIB_Type)sib_Type[0] = 5
. . . . . . (IntegerType)segmentIndex[-1] = 1
. . . . . . (BitStringType)sib_Data_fixed[222] = "000011111111010000000000000000001101011000110100010000111111010011100101000001100001000011001010000000110000001110001001000000010110000000000000100000001110000000001000100001100100001010011001000010100000000000110000000100"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 25 02 01 00 02 01 ff 00 04 50 0f f4 00 00 d6 34 43 f4 e5 06 10 ca 03 03 89 01 60 00 80 e0 08 86 42 99 0a 00 30 10

- No.: 503
- Timestamp: 12:20:46:608_0
- RFN: 426
- Chip: 26368
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 21
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 15

- No.: 508
- Timestamp: 12:20:46:616_0
- RFN: 427
- Chip: 20992
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB5_LongNeighCellInfo LINE 50
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 510
- Timestamp: 12:20:46:617_0
- RFN: 427
- Chip: 24320
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB5_LongNeighCellInfo LINE 52
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . LastSegmentShort
. . . . . . (SIB_Type)sib_Type[0] = 5
. . . . . . (IntegerType)segmentIndex[-1] = 2
. . . . . . (BitStringType)sib_Data_variable[-1] = "010001011100101011010110100000000000011110001000011000000001011011011011011000100000000001000011000010001001010000001011011010000000010000"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 1c 02 01 00 02 01 ff 00 06 51 89 45 ca d6 80 07 88 60 16 db 62 00 43 08 94 0b 68 04 00

- No.: 527
- Timestamp: 12:20:46:620_4
- RFN: 427
- Chip: 36864
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 2
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 02

- No.: 532
- Timestamp: 12:20:46:636_0
- RFN: 429
- Chip: 20736
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB6_LongNeighCellInfo LINE 8
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 535
- Timestamp: 12:20:46:637_0
- RFN: 429
- Chip: 24576
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB6_LongNeighCellInfo:lt_CompleteSIB LINE 4
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 6
. . . . . . . (BitStringType)sib_Data_variable[-1] = "0000001010010001"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 0c 02 01 00 02 01 ff 00 0e 06 0f 02 91

- No.: 540
- Timestamp: 12:20:46:638_3
- RFN: 429
- Chip: 29184
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 3
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 03

- No.: 545
- Timestamp: 12:20:46:646_0
- RFN: 430
- Chip: 19200
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB6_LongNeighCellInfo LINE 11
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 546
- Timestamp: 12:20:46:646_1
- RFN: 430
- Chip: 22016
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB6_LongNeighCellInfo LINE 12
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 08 02 01 00 02 01 ff 00 00

- No.: 550
- Timestamp: 12:20:46:647_3
- RFN: 430
- Chip: 25856
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 5
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 05

- No.: 555
- Timestamp: 12:20:46:656_0
- RFN: 431
- Chip: 20736
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB6_LongNeighCellInfo LINE 14
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 556
- Timestamp: 12:20:46:657_0
- RFN: 431
- Chip: 23296
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB6_LongNeighCellInfo LINE 15
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 08 02 01 00 02 01 ff 00 00

- No.: 560
- Timestamp: 12:20:46:658_0
- RFN: 431
- Chip: 26624
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 6
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 06

- No.: 565
- Timestamp: 12:20:46:666_0
- RFN: 432
- Chip: 19968
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB6_LongNeighCellInfo LINE 17
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 566
- Timestamp: 12:20:46:667_0
- RFN: 432
- Chip: 22784
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB6_LongNeighCellInfo LINE 18
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 08 02 01 00 02 01 ff 00 00

- No.: 574
- Timestamp: 12:20:46:670_0
- RFN: 432
- Chip: 36608
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 15
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 0f

- No.: 579
- Timestamp: 12:20:46:676_0
- RFN: 433
- Chip: 22528
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB7_LongNeighCellInfo LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 583
- Timestamp: 12:20:46:678_0
- RFN: 433
- Chip: 27904
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB7_LongNeighCellInfo:lt_CompleteSIB7OrLastSIB12_CompleteSIB7 LINE 9
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 7
. . . . . . . (BitStringType)sib_Data_variable[-1] = "100000101000000010000001"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 0d 02 01 00 02 01 ff 00 0e 07 17 82 80 81

- No.: 591
- Timestamp: 12:20:46:680_3
- RFN: 433
- Chip: 37888
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 7
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 07

- No.: 596
- Timestamp: 12:20:46:687_0
- RFN: 434
- Chip: 23296
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB7_LongNeighCellInfo:lt_ConcatWithSIB3 LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 597
- Timestamp: 12:20:46:687_1
- RFN: 434
- Chip: 26368
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB7_LongNeighCellInfo:lt_ConcatWithSIB3 LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 7
. . . . . . . (BitStringType)sib_Data_variable[-1] = "100000101000000010000001"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 3
. . . . . . . (BitStringType)sib_Data_variable[-1] = "010000000000000000000000000000001011001100011000010000000000001000000100011111111111111111111111"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 1b 02 01 00 02 01 ff 00 0e 27 17 82 80 81 1a fa 00 00 00 05 98 c2 00 10 23 ff ff f8

- No.: 605
- Timestamp: 12:20:46:690_0
- RFN: 434
- Chip: 36096
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 23
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 17

- No.: 610
- Timestamp: 12:20:46:706_0
- RFN: 436
- Chip: 19968
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB7_LongNeighCellInfo:lt_ConcatWithSIB18 LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 611
- Timestamp: 12:20:46:707_0
- RFN: 436
- Chip: 23552
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB7_LongNeighCellInfo:lt_ConcatWithSIB18 LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 7
. . . . . . . (BitStringType)sib_Data_variable[-1] = "100000101000000010000001"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 26
. . . . . . . (BitStringType)sib_Data_variable[-1] = "100010000111000000000010000010001100000000001000001000110000000000100000100011000000000011000100001"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 1b 02 01 00 02 01 ff 00 0e 27 17 82 80 81 d3 14 43 80 10 46 00 41 18 01 04 60 06 21

- No.: 619
- Timestamp: 12:20:46:709_1
- RFN: 436
- Chip: 33536
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 31
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 1f

- No.: 624
- Timestamp: 12:20:46:716_0
- RFN: 437
- Chip: 23296
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB7_LongNeighCellInfo:lt_ConcatWithSIB4 LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 625
- Timestamp: 12:20:46:717_0
- RFN: 437
- Chip: 26880
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB7_LongNeighCellInfo:lt_ConcatWithSIB4 LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 7
. . . . . . . (BitStringType)sib_Data_variable[-1] = "100000101000000010000001"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 4
. . . . . . . (BitStringType)sib_Data_variable[-1] = "0000000000000000000000000000000101100110001100001000000000000100000010001110111"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 19 02 01 00 02 01 ff 00 0e 27 17 82 80 81 22 70 00 00 00 0b 31 84 00 20 47 70

- No.: 639
- Timestamp: 12:20:46:721_2
- RFN: 438
- Chip: 3584
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 30
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 1e

- No.: 644
- Timestamp: 12:20:46:727_0
- RFN: 438
- Chip: 24064
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB11_LongNeighCellInfo LINE 41
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 645
- Timestamp: 12:20:46:727_1
- RFN: 438
- Chip: 26624
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB11_LongNeighCellInfo LINE 42
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 08 02 01 00 02 01 ff 00 00

- No.: 649
- Timestamp: 12:20:46:728_3
- RFN: 438
- Chip: 30464
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 27
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 1b

- No.: 654
- Timestamp: 12:20:46:736_0
- RFN: 439
- Chip: 20480
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB11_LongNeighCellInfo LINE 44
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 655
- Timestamp: 12:20:46:736_1
- RFN: 439
- Chip: 23296
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB11_LongNeighCellInfo LINE 45
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . SubsequentSegment
. . . . . . (SIB_Type)sib_Type[0] = 11
. . . . . . (IntegerType)segmentIndex[-1] = 1
. . . . . . (BitStringType)sib_Data_fixed[222] = "101000100000101000010000110000100101001001101010100001100001001010100100110001101100101101111111010010111010100101001100100000110110010100011100110100000000010001000010101001011000011011001010001110011010000000001000101001"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 25 02 01 00 02 01 ff 00 04 b0 a2 0a 10 c2 52 6a 86 12 a4 c6 cb 7f 4b a9 4c 83 65 1c d0 04 42 a5 86 ca 39 a0 08 a4

- No.: 659
- Timestamp: 12:20:46:738_0
- RFN: 439
- Chip: 28160
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 26
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 1a

- No.: 664
- Timestamp: 12:20:46:746_0
- RFN: 440
- Chip: 20224
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB11_LongNeighCellInfo LINE 47
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 665
- Timestamp: 12:20:46:746_1
- RFN: 440
- Chip: 23296
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB11_LongNeighCellInfo LINE 48
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . FirstSegment
. . . . . . (SIB_Type)sib_Type[0] = 11
. . . . . . (IntegerType)seg_Count[-1] = 3
. . . . . . (BitStringType)sib_Data_fixed[222] = "001000001101100100001010000000001000110010000100001001010010010110101101100101000111001101000000000100010001010011001000101101100101000111001101000000000000100010001000110010010101010000000100101000010100101010000110000100"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 25 02 01 00 02 01 ff 00 02 b2 20 d9 0a 00 8c 84 25 25 ad 94 73 40 11 14 c8 b6 51 cd 00 08 88 c9 54 04 a1 4a 86 10

- No.: 669
- Timestamp: 12:20:46:748_0
- RFN: 440
- Chip: 27392
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 29
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 1d

- No.: 674
- Timestamp: 12:20:46:756_0
- RFN: 441
- Chip: 20736
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB11_LongNeighCellInfo LINE 50
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 676
- Timestamp: 12:20:46:757_0
- RFN: 441
- Chip: 24064
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB11_LongNeighCellInfo LINE 52
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . LastSegmentShort
. . . . . . (SIB_Type)sib_Type[0] = 11
. . . . . . (IntegerType)segmentIndex[-1] = 2
. . . . . . (BitStringType)sib_Data_variable[-1] = "01010101111000110110010100011100110100000000011001100110010111110001101001101001110010100100101100011011001010001110011010000000001000111001010111000010001101100101000111001101000000000"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 22 02 01 00 02 01 ff 00 06 b1 b8 55 e3 65 1c d0 06 66 5f 1a 69 ca 4b 1b 28 e6 80 23 95 c2 36 51 cd 00 00

- No.: 689
- Timestamp: 12:20:46:760_1
- RFN: 441
- Chip: 37632
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 13
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 0d

- No.: 694
- Timestamp: 12:20:46:776_0
- RFN: 443
- Chip: 20736
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB12_LongNeighCellInfo LINE 41
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 695
- Timestamp: 12:20:46:776_1
- RFN: 443
- Chip: 23808
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB12_LongNeighCellInfo LINE 42
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . SubsequentSegment
. . . . . . (SIB_Type)sib_Type[0] = 12
. . . . . . (IntegerType)segmentIndex[-1] = 1
. . . . . . (BitStringType)sib_Data_fixed[222] = "110000100101001001101010100001100001001010100100110001101100101101111111010010111010100101001100100010110110010100011100110100000000010001000010101001011001011011001010001110011010000000001000101001010101011110101101100101"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 25 02 01 00 02 01 ff 00 04 c0 c2 52 6a 86 12 a4 c6 cb 7f 4b a9 4c 8b 65 1c d0 04 42 a5 96 ca 39 a0 08 a5 57 ad 94

- No.: 699
- Timestamp: 12:20:46:778_0
- RFN: 443
- Chip: 29184
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 11
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 0b

- No.: 704
- Timestamp: 12:20:46:785_0
- RFN: 444
- Chip: 19200
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB12_LongNeighCellInfo LINE 44
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 705
- Timestamp: 12:20:46:786_0
- RFN: 444
- Chip: 22272
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB12_LongNeighCellInfo LINE 45
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . FirstSegment
. . . . . . (SIB_Type)sib_Type[0] = 12
. . . . . . (IntegerType)seg_Count[-1] = 3
. . . . . . (BitStringType)sib_Data_fixed[222] = "000000011011001000001100001001010010010110101101100101000111001101000000000100010001010011001000101101100101000111001101000000000000100010001000110010010101010000000100101000010100100000000110000100101000100000101000010000"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 25 02 01 00 02 01 ff 00 02 c2 01 b2 0c 25 25 ad 94 73 40 11 14 c8 b6 51 cd 00 08 88 c9 54 04 a1 48 06 12 88 28 40

- No.: 709
- Timestamp: 12:20:46:787_1
- RFN: 444
- Chip: 26368
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 15
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 0f

- No.: 714
- Timestamp: 12:20:46:796_0
- RFN: 445
- Chip: 20736
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB12_LongNeighCellInfo LINE 47
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 719
- Timestamp: 12:20:46:797_2
- RFN: 445
- Chip: 27904
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB12_LongNeighCellInfo:lt_CompleteSIB7 LINE 7
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 7
. . . . . . . (BitStringType)sib_Data_variable[-1] = "100000101000000010000001"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 0d 02 01 00 02 01 ff 00 0e 07 17 82 80 81

- No.: 724
- Timestamp: 12:20:46:799_0
- RFN: 445
- Chip: 32256
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 14
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 0e

- No.: 729
- Timestamp: 12:20:46:806_0
- RFN: 446
- Chip: 23040
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB12_LongNeighCellInfo LINE 50
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 731
- Timestamp: 12:20:46:807_0
- RFN: 446
- Chip: 26624
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB12_LongNeighCellInfo LINE 52
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . LastSegmentShort
. . . . . . (SIB_Type)sib_Type[0] = 12
. . . . . . (IntegerType)segmentIndex[-1] = 2
. . . . . . (BitStringType)sib_Data_variable[-1] = "00011100110100000000011001100110010111110001101001101001110010100100101101011011001010001110011010000000001000111001010111000010101101100101000111001101000000000"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 1f 02 01 00 02 01 ff 00 06 c1 a0 1c d0 06 66 5f 1a 69 ca 4b 5b 28 e6 80 23 95 c2 b6 51 cd 00 00

- No.: 739
- Timestamp: 12:20:46:810_0
- RFN: 446
- Chip: 38144
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 23
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 06 02 01 17

- No.: 744
- Timestamp: 12:20:46:816_0
- RFN: 447
- Chip: 24064
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB18_LongNeighCellInfo LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 745
- Timestamp: 12:20:46:817_0
- RFN: 447
- Chip: 27136
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB18_LongNeighCellInfo LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 7
. . . . . . . (BitStringType)sib_Data_variable[-1] = "100000101000000010000001"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 26
. . . . . . . (BitStringType)sib_Data_variable[-1] = "100010000111000000000010000010001100000000001000001000110000000000100000100011000000000011000100001"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 1b 02 01 00 02 01 ff 00 0e 27 17 82 80 81 d3 14 43 80 10 46 00 41 18 01 04 60 06 21

- No.: 757
- Timestamp: 12:20:46:820_0
- RFN: 447
- Chip: 37632
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 4
. . (IntegerType)sg_POS[-1] = 1
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 04 02 01 01

- No.: 762
- Timestamp: 12:20:46:835_0
- RFN: 449
- Chip: 20736
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSB1_LongNeighCellInfo LINE 4
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 765
- Timestamp: 12:20:46:836_2
- RFN: 449
- Chip: 24576
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSB1_LongNeighCellInfo:lt_CompleteSIB LINE 4
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 27
. . . . . . . (BitStringType)sib_Data_variable[-1] = "0001000010101000100000100011000001011101010011100100100110100001000000010101101110010010001011000100010000110010100010010111"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 1a 02 01 00 02 01 ff 00 0e 1b 7b 10 a8 82 30 5d 4e 49 a1 01 5b 92 2c 44 32 89 70

- No.: 783
- Timestamp: 12:20:46:840_1
- RFN: 450
- Chip: 0
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 3
. . (IntegerType)sg_POS[-1] = 0
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 00 02 01 ff 0a 01 00 30 06 02 01 03 02 01 00

- No.: 788
- Timestamp: 12:20:46:856_0
- RFN: 451
- Chip: 20992
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendMIB LINE 7
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 791
- Timestamp: 12:20:46:858_0
- RFN: 451
- Chip: 25600
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendMIB:lt_CompleteSIB LINE 4
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 0
. . . . . . . (BitStringType)sib_Data_variable[-1] = "0000000000000000010000000010010110101010000100010000000000001000100010100000101000100010100001001000100001110001101000100111110010001110010010010010000100000001"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 1e 02 01 00 02 01 ff 00 0e 00 9f 00 00 40 25 aa 11 00 08 8a 0a 22 84 88 71 a2 7c 8e 49 21 01

- No.: 798
- Timestamp: 12:20:46:859_1
- RFN: 451
- Chip: 29696
- Event: Start Timer
- Source: ts_RRC_Delay LINE 1
- Message Structure:
no details available
- Constraint:
t_Dly (5000 Ms)
- BinaryMessage:

- No.: 802
- Timestamp: 12:20:51:848_0
- RFN: 950
- Chip: 33024
- Event: Timeout
- Source: ts_RRC_Delay LINE 2
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 814
- Timestamp: 12:20:51:850_0
- RFN: 951
- Chip: 3328
- Event: Send
- PCO: CMAC
- Message: CMAC_PAGING_Config_REQ
- Source: ts_CMAC_Pag1_Cfg LINE 4
- Message Structure:
CMAC_PAGING_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 5
. (RatType)ratType[0] = 0
. CmacPagingConfigReq
. . pI_BitMapInfo
. . . (BitStringType)e18[18] = '010000000000000000'B
. . (IntegerType)dRX_CycleLength[-1] = 7
. . IMSI_GSM_MAP
. . . (IntegerType)_elem[-1] = 0
. . . (IntegerType)_elem[-1] = 0
. . . (IntegerType)_elem[-1] = 1
. . . (IntegerType)_elem[-1] = 0
. . . (IntegerType)_elem[-1] = 1
. . . (IntegerType)_elem[-1] = 0
. . . (IntegerType)_elem[-1] = 1
. . . (IntegerType)_elem[-1] = 2
. . . (IntegerType)_elem[-1] = 3
. . . (IntegerType)_elem[-1] = 4
. . . (IntegerType)_elem[-1] = 5
. . . (IntegerType)_elem[-1] = 6
. . . (IntegerType)_elem[-1] = 0
. . . (IntegerType)_elem[-1] = 6
. . . (IntegerType)_elem[-1] = 3
. . (BooleanType)t_pich_T_sccpch = FALSE
- Constraint:
ca_CMAC_PagingCfgReq
- BinaryMessage:
30 46 02 01 00 02 01 05 0a 01 00 30 3b 03 04 06 40 40 40 02 01 07 30 2d 02 01 00 02 01 00 02 01 01 02 01 00 02 01 01 02 01 00 02 01 01 02 01 02 02 01 03 02 01 04 02 01 05 02 01 06 02 01 00 02 01 06 02 01 03 01 01 00

- No.: 818
- Timestamp: 12:20:51:855_0
- RFN: 951
- Chip: 22528
- Event: Receive
- PCO: CMAC
- Message: CMAC_PAGING_Config_CNF
- Source: ts_CMAC_Pag1_Cfg LINE 5
- Message Structure:
CMAC_PAGING_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 5
- Constraint:
ca_CMAC_PagingCfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 05

- No.: 820
- Timestamp: 12:20:51:856_1
- RFN: 951
- Chip: 25856
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendPage1_ModifySI LINE 3
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -2
. tM_message
. . PCCH_Message
. . . PCCH_MessageType
. . . . PagingType1
. . . . . PagingRecordList
. . . . . BCCH_ModificationInfo
. . . . . . (IntegerType)mib_ValueTag[-1] = 1
. . . . . . (IntegerType)bcch_ModificationTime[-1] = -
. . . . . laterNonCriticalExtensions
- Constraint:
cas_PagingType1
- BinaryMessage:
30 07 02 01 00 02 01 fe 20

- No.: 827
- Timestamp: 12:20:51:858_0
- RFN: 951
- Chip: 30976
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSysInfoChangeInd_InFACHConfig LINE 3
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -3
. tM_message
. . BCCH_FACH_Message
. . . BCCH_FACH_MessageType
. . . . SystemInformationChangeIndication
. . . . . BCCH_ModificationInfo
. . . . . . (IntegerType)mib_ValueTag[-1] = 1
. . . . . . (IntegerType)bcch_ModificationTime[-1] = -
. . . . . laterNonCriticalExtensions
- Constraint:
cas_SysInfoChangeInd
- BinaryMessage:
30 07 02 01 00 02 01 fd 40

- No.: 838
- Timestamp: 12:20:51:859_4
- RFN: 951
- Chip: 37376
- Event: Send
- PCO: Ut
- Message: MMI_CmdReq
- Source: ts_MMI_Cmd LINE 1
- Message Structure:
MMI_CmdReq
. (IA5StringType)cmd[-1] = "Please switch on the UE"
- Constraint:
ca_MMI_CmdReq
- BinaryMessage:
50 6c 65 61 73 65 20 73 77 69 74 63 68 20 6f 6e 20 74 68 65 20 55 45

- No.: 842
- Timestamp: 12:20:53:063_0
- RFN: 1072
- Chip: 12544
- Event: Receive
- PCO: Ut
- Message: MMI_CmdCnf
- Source: ts_MMI_Cmd LINE 2
- Message Structure:
MMI_CmdCnf
. (BooleanType)result = TRUE
. (IA5StringType)resultString[0] = ""
- Constraint:
ca_MMI_CmdCnf
- BinaryMessage:
80

- No.: 856
- Timestamp: 12:20:53:065_3
- RFN: 1072
- Chip: 22016
- Event: Send
- PCO: Ut
- Message: MMI_CmdReq
- Source: ts_MMI_UE_SwitchOn LINE 2
- Message Structure:
MMI_CmdReq
. (IA5StringType)cmd[-1] = "Please switch on the UE"
- Constraint:
ca_MMI_CmdReq
- BinaryMessage:
50 6c 65 61 73 65 20 73 77 69 74 63 68 20 6f 6e 20 74 68 65 20 55 45

- No.: 860
- Timestamp: 12:20:57:904_0
- RFN: 1556
- Chip: 15104
- Event: Receive
- PCO: Ut
- Message: MMI_CmdCnf
- Source: ts_MMI_UE_SwitchOn LINE 3
- Message Structure:
MMI_CmdCnf
. (BooleanType)result = TRUE
. (IA5StringType)resultString[0] = ""
- Constraint:
ca_MMI_CmdCnf
- BinaryMessage:
80

- No.: 865
- Timestamp: 12:20:57:904_5
- RFN: 1556
- Chip: 17920
- Event: Start Timer
- Source: ts_MM_IdleUpdated LINE 3
- Message Structure:
no details available
- Constraint:
t_Dly (35000 Ms)
- BinaryMessage:

- No.: 883
- Timestamp: 12:21:03:785_0
- RFN: 2144
- Chip: 21760
- Event: Receive
- PCO: TM
- Message: RLC_TR_DATA_IND
- Source: ts_RRC_ConnEst:lt_RcvConnReq LINE 2
- Message Structure:
RLC_TR_DATA_IND
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 0
. tM_message
. . UL_CCCH_Message
. . . IntegrityCheckInfo
. . . UL_CCCH_MessageType
. . . . RRCConnectionRequest
. . . . . InitialUE_Identity
. . . . . . TMSI_and_LAI_GSM_MAP
. . . . . . . (BitStringType)tmsi[32] = "00010010001101000101011001111000"
. . . . . . . LAI
. . . . . . . . PLMN_Identity
. . . . . . . . . MCC
. . . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . . (IntegerType)_elem[4] = 1
. . . . . . . . . MNC
. . . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . . (IntegerType)_elem[4] = 1
. . . . . . . . (BitStringType)lac[16] = '0000000000000001'B
. . . . . (EstablishmentCause)establishmentCause[5] = 12
. . . . . (ProtocolErrorIndicator)protocolErrorIndicator[1] = 0
. . . . . MeasuredResultsOnRACH
. . . . . v3d0NonCriticalExtensions
- Constraint:
car_RRC_ConnReq
- BinaryMessage:
30 11 02 01 00 02 01 00 21 12 34 56 78 00 10 08 00 0b 00

- No.: 887
- Timestamp: 12:21:03:790_0
- RFN: 2145
- Chip: 2048
- Event: Send
- PCO: UM
- Message: RLC_UM_DATA_REQ
- Source: ts_RRC_ConnEst:lt_Send_ConnSetUp LINE 2
- Message Structure:
RLC_UM_DATA_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 0
. uM_message
. . DL_CCCH_Message
. . . IntegrityCheckInfo
. . . DL_CCCH_MessageType
. . . . RRCConnectionSetup
. . . . . r3
. . . . . . RRCConnectionSetup_r3_IEs
. . . . . . . InitialUE_Identity
. . . . . . . . TMSI_and_LAI_GSM_MAP
. . . . . . . . . (BitStringType)tmsi[32] = "00010010001101000101011001111000"
. . . . . . . . . LAI
. . . . . . . . . . PLMN_Identity
. . . . . . . . . . . MCC
. . . . . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . . . . (IntegerType)_elem[4] = 1
. . . . . . . . . . . MNC
. . . . . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . . . . (IntegerType)_elem[4] = 1
. . . . . . . . . . (BitStringType)lac[16] = '0000000000000001'B
. . . . . . . (IntegerType)rrc_TransactionIdentifier[-1] = 0
. . . . . . . (IntegerType)activationTime[-1] = -
. . . . . . . U_RNTI
. . . . . . . . (BitStringType)srnc_Identity[12] = "000000000001"
. . . . . . . . (BitStringType)s_RNTI[20] = "00000000000000000001"
. . . . . . . (BitStringType)new_c_RNTI[16] = "0000000000000001"
. . . . . . . (RRC_StateIndicator)rrc_StateIndicator[0] = 1
. . . . . . . (IntegerType)utran_DRX_CycleLengthCoeff[-1] = 9
. . . . . . . CapabilityUpdateRequirement
. . . . . . . . (BooleanType)ue_RadioCapabilityFDDUpdateRequirement = TRUE
. . . . . . . . (BooleanType)ue_RadioCapabilityTDDUpdateRequirement = FALSE
. . . . . . . . SystemSpecificCapUpdateReqList
. . . . . . . . . (SystemSpecificCapUpdateReq)_elem[0] = 0
. . . . . . . SRB_InformationSetupList2
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity[-1] = 1
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_UM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (NoExplicitDiscard)timerBasedNoExplicit[0] = 4
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex[-1] = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 1
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 1
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity[-1] = 2
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 2
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex[-1] = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 2
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 2
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 2
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 2
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 2
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity[-1] = 3
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 3
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex[-1] = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 3
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 3
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 3
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 3
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 3
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity[-1] = 4
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 4
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex[-1] = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 4
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 4
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 4
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 4
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 4
. . . . . . . UL_CommonTransChInfo
. . . . . . . . TFC_Subset
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . TFCS
. . . . . . . . . . . ExplicitTFCS_Configuration
. . . . . . . . . . . . TFCS_ReconfAdd
. . . . . . . . . . . . . ctfcSize
. . . . . . . . . . . . . . ctfc2Bit
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . . . . . . . (IntegerType)ctfc2[-1] = 0
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . . . . . . . (IntegerType)ctfc2[-1] = 1
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC[-1] = 11
. . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaD[-1] = 15
. . . . . . . . . . . . . . . . . . . (IntegerType)referenceTFC_ID[-1] = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . UL_AddReconfTransChInfoList
. . . . . . . . UL_AddReconfTransChInformation
. . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType[0] = 0
. . . . . . . . . (IntegerType)transportChannelIdentity[-1] = 5
. . . . . . . . . TransportFormatSet
. . . . . . . . . . DedicatedTransChTFS
. . . . . . . . . . . tti
. . . . . . . . . . . . DedicatedDynamicTF_InfoList
. . . . . . . . . . . . . DedicatedDynamicTF_Info
. . . . . . . . . . . . . . rlc_Size
. . . . . . . . . . . . . . . BitModeRLC_SizeInfo
. . . . . . . . . . . . . . . . sizeType2
. . . . . . . . . . . . . . . . . (IntegerType)part1[-1] = 2
. . . . . . . . . . . . . . . . . (IntegerType)part2[-1] = -
. . . . . . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . LogicalChannelList
. . . . . . . . . . . SemistaticTF_Information
. . . . . . . . . . . . ChannelCodingType
. . . . . . . . . . . . . (CodingRate)convolutional[0] = 1
. . . . . . . . . . . . (IntegerType)rateMatchingAttribute[-1] = 170
. . . . . . . . . . . . (CRC_Size)crc_Size[0] = 3
. . . . . . . DL_CommonTransChInfo
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . dl_Parameters
. . . . . . . DL_AddReconfTransChInfoList
. . . . . . . . DL_AddReconfTransChInformation
. . . . . . . . . (DL_TrCH_Type)dl_TransportChannelType[0] = 0
. . . . . . . . . (IntegerType)dl_transportChannelIdentity[-1] = 10
. . . . . . . . . tfs_SignallingMode
. . . . . . . . . . UL_TransportChannelIdentity
. . . . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType[0] = 0
. . . . . . . . . . . (IntegerType)ul_TransportChannelIdentity[-1] = 5
. . . . . . . . . QualityTarget
. . . . . . . . . . (IntegerType)bler_QualityValue[-1] = -20
. . . . . . . . . TM_SignallingInfo
. . . . . . . FrequencyInfo
. . . . . . . (IntegerType)maxAllowedUL_TX_Power[-1] = -
. . . . . . . UL_ChannelRequirement
. . . . . . . DL_CommonInformation
. . . . . . . DL_InformationPerRL_List
. . . . . . laterNonCriticalExtensions
. (BooleanType)specialLI = TRUE
- Constraint:
cas_RRC_ConnSetup
- BinaryMessage:
30 6c 02 01 00 02 01 00 31 e0 22 46 8a cf 00 02 01 00 01 00 04 00 00 40 00 5d 83 03 6a 27 50 80 00 a1 a1 01 08 90 85 9e 8e 46 c9 a6 7c 9c 4e 75 18 00 2a 3a 10 52 89 18 99 e8 e4 6c 9a 67 c9 c4 e7 52 80 04 a5 a1 09 48 92 8d 9e 8e 46 c9 a6 7c 9c 4e 75 38 00 6a 7a 10 d6 89 32 00 01 89 4a fc 00 84 02 20 88 ea 59 82 26 25 60 01 01 ff

- No.: 908
- Timestamp: 12:21:03:812_0
- RFN: 2147
- Chip: 8704
- Event: Start Timer
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 8
- Message Structure:
no details available
- Constraint:
t_WaitMS (13500 Ms)
- BinaryMessage:

- No.: 914
- Timestamp: 12:21:04:157_0
- RFN: 2181
- Chip: 28928
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_IND
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 10
- Message Structure:
RLC_AM_DATA_IND
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
. IntegrityResult
. . (IntegrityStatus)integrityUsed[0] = 4294967296
. aM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . UL_DCCH_MessageType
. . . . RRCConnectionSetupComplete
. . . . . (IntegerType)rrc_TransactionIdentifier[2] = 0
. . . . . STARTList
. . . . . . STARTSingle
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity[1] = 0
. . . . . . . (BitStringType)start_Value[20] = "00000000000000000010"
. . . . . . STARTSingle
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity[1] = 1
. . . . . . . (BitStringType)start_Value[20] = "00000000000000000010"
. . . . . UE_RadioAccessCapability
. . . . . . (AccessStratumReleaseIndicator)accessStratumReleaseIndicator[0] = 0
. . . . . . PDCP_Capability
. . . . . . . (BooleanType)losslessSRNS_RelocationSupport = FALSE
. . . . . . . supportForRfc2507
. . . . . . RLC_Capability
. . . . . . . (TotalRLC_AM_BufferSize)totalRLC_AM_BufferSize[3] = 2
. . . . . . . (MaximumRLC_WindowSize)maximumRLC_WindowSize[1] = 0
. . . . . . . (MaximumAM_EntityNumberRLC_Cap)maximumAM_EntityNumber[3] = 3
. . . . . . TransportChannelCapability
. . . . . . . DL_TransChCapability
. . . . . . . . (MaxNoBits)maxNoBitsReceived[4] = 5
. . . . . . . . (MaxNoBits)maxConvCodeBitsReceived[4] = 0
. . . . . . . . TurboSupport
. . . . . . . . . (MaxNoBits)supported[4] = 5
. . . . . . . . (MaxSimultaneousTransChsDL)maxSimultaneousTransChs[2] = 1
. . . . . . . . (IntegerType)maxSimultaneousCCTrCH_Count[3] = 1
. . . . . . . . (MaxTransportBlocksDL)maxReceivedTransportBlocks[4] = 3
. . . . . . . . (MaxNumberOfTFC_DL)maxNumberOfTFC[4] = 5
. . . . . . . . (MaxNumberOfTF)maxNumberOfTF[3] = 1
. . . . . . . UL_TransChCapability
. . . . . . . . (MaxNoBits)maxNoBitsTransmitted[4] = 3
. . . . . . . . (MaxNoBits)maxConvCodeBitsTransmitted[4] = 0
. . . . . . . . TurboSupport
. . . . . . . . . (MaxNoBits)supported[4] = 3
. . . . . . . . (MaxSimultaneousTransChsUL)maxSimultaneousTransChs[3] = 2
. . . . . . . . modeSpecificInfo
. . . . . . . . (MaxTransportBlocksUL)maxTransmittedBlocks[4] = 2
. . . . . . . . (MaxNumberOfTFC_UL)maxNumberOfTFC[4] = 3
. . . . . . . . (MaxNumberOfTF)maxNumberOfTF[3] = 0
. . . . . . RF_Capability
. . . . . . . fddRF_Capability
. . . . . . . . (IntegerType)ue_PowerClass[2] = 4
. . . . . . . . (TxRxFrequencySeparation)txRxFrequencySeparation[2] = 0
. . . . . . . tddRF_Capability
. . . . . . PhysicalChannelCapability
. . . . . . . fddPhysChCapability
. . . . . . . . DL_PhysChCapabilityFDD
. . . . . . . . . (IntegerType)maxNoDPCH_PDSCH_Codes[3] = 3
. . . . . . . . . (MaxNoPhysChBitsReceived)maxNoPhysChBitsReceived[4] = 8
. . . . . . . . . (BooleanType)supportForSF_512 = FALSE
. . . . . . . . . (BooleanType)supportOfPDSCH = FALSE
. . . . . . . . . SimultaneousSCCPCH_DPCH_Reception
. . . . . . . . UL_PhysChCapabilityFDD
. . . . . . . . . (MaxNoDPDCH_BitsTransmitted)maxNoDPDCH_BitsTransmitted[4] = 2
. . . . . . . . . (BooleanType)supportOfPCPCH = FALSE
. . . . . . . tddPhysChCapability
. . . . . . UE_MultiModeRAT_Capability
. . . . . . . MultiRAT_Capability
. . . . . . . . (BooleanType)supportOfGSM = FALSE
. . . . . . . . (BooleanType)supportOfMulticarrier = FALSE
. . . . . . . (MultiModeCapability)multiModeCapability[2] = 1
. . . . . . SecurityCapability
. . . . . . . (BitStringType)cipheringAlgorithmCap[16] = '0000000000000011'B
. . . . . . . (BitStringType)integrityProtectionAlgorithmCap[16] = '0000000000000010'B
. . . . . . UE_Positioning_Capability
. . . . . . . (BooleanType)standaloneLocMethodsSupported = FALSE
. . . . . . . (BooleanType)ue_BasedOTDOA_Supported = FALSE
. . . . . . . (NetworkAssistedGPS_Supported)networkAssistedGPS_Supported[2] = 3
. . . . . . . (BooleanType)supportForUE_GPS_TimingOfCellFrames = FALSE
. . . . . . . (BooleanType)supportForIPDL = FALSE
. . . . . . MeasurementCapability
. . . . . . . CompressedModeMeasCapability
. . . . . . . . (BooleanType)fdd_Measurements = FALSE
. . . . . . . . (BooleanType)tdd_Measurements = -
. . . . . . . . GSM_Measurements
. . . . . . . . . (BooleanType)gsm900 = FALSE
. . . . . . . . . (BooleanType)dcs1800 = FALSE
. . . . . . . . . (BooleanType)gsm1900 = FALSE
. . . . . . . . (BooleanType)multiCarrierMeasurements = -
. . . . . . . CompressedModeMeasCapability
. . . . . . . . (BooleanType)fdd_Measurements = FALSE
. . . . . . . . (BooleanType)tdd_Measurements = -
. . . . . . . . GSM_Measurements
. . . . . . . . . (BooleanType)gsm900 = FALSE
. . . . . . . . . (BooleanType)dcs1800 = FALSE
. . . . . . . . . (BooleanType)gsm1900 = FALSE
. . . . . . . . (BooleanType)multiCarrierMeasurements = -
. . . . . v370NonCriticalExtensions
- Constraint:
car_RRC_ConnSetupCmpl
- BinaryMessage:
30 27 02 01 ff 02 01 02 0a 05 01 00 00 00 00 4a 08 00 00 a0 00 05 11 a8 55 06 a4 c2 68 46 2c 94 02 08 00 18 00 11 88 10 00

- No.: 915
- Timestamp: 12:21:04:159_0
- RFN: 2181
- Chip: 36352
- Event: Cancel Timer
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 10
- Message Structure:
no details available
- Constraint:
t_WaitMS
- BinaryMessage:

- No.: 916
- Timestamp: 12:21:04:159_1
- RFN: 2181
- Chip: 36608
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 10
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 934
- Timestamp: 12:21:04:355_0
- RFN: 2201
- Chip: 25088
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_MM_IdleUpdated LINE 5
- Message Structure:
RRC_DataInd
. (IntegerType)cellId[0] = -1
. (SS_RB_Identity)rB_Id[0] = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain[0] = 0
. (START_Value)start[20] = '00000000000000000000'B
. LOCATIONUPDATINGREQUEST
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)mMProtocolDiscriminator[4] = '0101'B
. . (MsgType)msgType[8] = '00001000'B
. . CiphKeySeqNum
. . . (B1)spare1[1] = '0'B
. . . (KeySeq)keySeq[3] = '000'B
. . LocUpdType
. . . (B1)fOR[1] = '0'B
. . . (B1)spare1[1] = '0'B
. . . (B2)lUT[2] = '10'B
. . LocAreaId_v
. . . (OctetStringType)plmn[3] = '00F110'O
. . . (OctetStringType)lac[2] = '0001'O
. . MS_Clsmk1
. . . (B1)spare1[1] = '0'B
. . . (B2)revLvl[2] = '10'B
. . . (B1)eSIND[1] = '0'B
. . . (B1)a5_1[1] = '1'B
. . . (B3)rFPwrCap[3] = '111'B
. . MS_Identity_lv
. . . (Length)iel[1] = '05'O
. . . (B4)iDigit1[4] = '1111'B
. . . (B1)oddEvenInd[1] = '0'B
. . . (B3)typeOfId[3] = '100'B
. . . (OctetStringType)otherDigits[4] = '12345678'O
. . MS_Clsmk2
. . . (IEI8)iei[8] = '00110011'B
. . . (Length)iel[1] = '03'O
. . . (B1)spare1_1[1] = '0'B
. . . (B2)revLvl[2] = '10'B
. . . (B1)eSIND[1] = '0'B
. . . (B1)a5_1[1] = '1'B
. . . (B3)rFPwrCap[3] = '111'B
. . . (B1)spare1_2[1] = '0'B
. . . (B1)pSCap[1] = '0'B
. . . (B2)sSSI[2] = '01'B
. . . (B1)sMCap[1] = '1'B
. . . (B1)vBS[1] = '0'B
. . . (B1)vGCS[1] = '0'B
. . . (B1)fC[1] = '0'B
. . . (B1)cM3[1] = '1'B
. . . (B1)spare1_3[1] = '0'B
. . . (B1)lCSVA[1] = '0'B
. . . (B1)uCS2[1] = '0'B
. . . (B1)soLSA[1] = '0'B
. . . (B1)cMSP[1] = '0'B
. . . (B1)a5_3[1] = '0'B
. . . (B1)a5_2[1] = '0'B
- Constraint:
car_InitDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 00 03 04 04 00 00 00 05 08 02 00 f1 10 00 01 4f 05 f4 12 34 56 78 33 03 4f 18 80

- No.: 935
- Timestamp: 12:21:04:356_0
- RFN: 2201
- Chip: 27904
- Event: Cancel Timer
- Source: ts_MM_IdleUpdated LINE 5
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 971
- Timestamp: 12:21:04:362_0
- RFN: 2202
- Chip: 13824
- Event: Send
- PCO: Dc
- Message: RRC_DataReq
- Source: ts_MM_Authentication LINE 2
- Message Structure:
RRC_DataReq
. (IntegerType)cellId[-1] = -1
. (SS_RB_Identity)rB_Id[-1] = 3
. (LogicChGERAN)ch[-1] = -
. (SapId)sapId[1] = -
. (SS_CN_DomainIdentity)cN_Domain[-1] = 0
. AUTHENTICATIONREQUEST
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)mMProtocolDiscriminator[4] = '0101'B
. . (MsgType)msgType[8] = '00010010'B
. . (B4)spare4[4] = '0000'B
. . CiphKeySeqNum
. . . (B1)spare1[1] = '0'B
. . . (KeySeq)keySeq[3] = '000'B
. . (MM_RAND)rAND[128] = '01010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101'B
. . AUTN
. . . (IEI8)iei[8] = '00100000'B
. . . (Length)iel[1] = '10'O
. . . (BitStringType)aUTN[128] = '01010110010100010101000001010011010100100101110100000000000000000101010101010100010101110101011001010001010100000101001101010010'B
- Constraint:
ca_DataReq
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 00 05 12 00 55 55 55 55 55 55 55 55 55 55 55 55 55 55 55 55 20 10 56 51 50 53 52 5d 00 00 55 54 57 56 51 50 53 52

- No.: 975
- Timestamp: 12:21:05:165_0
- RFN: 2282
- Chip: 22784
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_MM_Authentication LINE 7
- Message Structure:
RRC_DataInd
. (IntegerType)cellId[0] = -1
. (SS_RB_Identity)rB_Id[0] = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain[0] = 0
. (START_Value)start[0] = -
. AUTHENTICATIONRESPONSE
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)mMProtocolDiscriminator[4] = '0101'B
. . (MsgType)msgType[8] = '01010100'B
. . (AuthRsp)authRsp[32] = '01010101010101000101011101010110'B
. . AuthRspExt
- Constraint:
car_UplinkDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 00 05 54 55 54 57 56

- No.: 1017
- Timestamp: 12:21:05:170_3
- RFN: 2283
- Chip: 5888
- Event: Send
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_REQ
- Source: ts_SS_DownloadSecurityKey:lt_DownloadKeyCRLC LINE 1
- Message Structure:
CRLC_SecurityMode_Config_REQ
. (IntegerType)cellId[-1] = -1
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity[0] = 0
. . (BitStringType)startValue[20] = "00000000000000000000"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = '01010111010101100101000101010000010100110101001001011101010111000101111101011110010110010101100001011011010110100101010101010100'B
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CRLC_SecurityModeCfgReq
- BinaryMessage:
30 21 02 01 ff 30 1c 0a 01 00 03 04 04 00 00 00 03 11 00 57 56 51 50 50 52 5d 5c 5c 5e 59 58 58 5a 55 54

- No.: 1018
- Timestamp: 12:21:05:171_0
- RFN: 2283
- Chip: 7680
- Event: Receive
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_CNF
- Source: ts_SS_DownloadSecurityKey:lt_DownloadKeyCRLC LINE 2
- Message Structure:
CRLC_SecurityMode_Config_CNF
. (IntegerType)cellId[0] = -1
- Constraint:
ca_CRLC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1025
- Timestamp: 12:21:05:172_0
- RFN: 2283
- Chip: 11776
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 1
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 0
. (IntegerType)count_I_LSB_UL[-1] = -
. (IntegerType)count_I_LSB_DL[-1] = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 00 02 01 00 02 01 00

- No.: 1026
- Timestamp: 12:21:05:172_1
- RFN: 2283
- Chip: 13312
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 2
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 0
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 00 02 01 00

- No.: 1027
- Timestamp: 12:21:05:173_0
- RFN: 2283
- Chip: 14848
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 3
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 1
. (IntegerType)count_I_LSB_UL[-1] = -
. (IntegerType)count_I_LSB_DL[-1] = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 01 02 01 00

- No.: 1028
- Timestamp: 12:21:05:173_1
- RFN: 2283
- Chip: 16384
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 4
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 1
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 1029
- Timestamp: 12:21:05:174_0
- RFN: 2283
- Chip: 18944
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 5
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 2
. (IntegerType)count_I_LSB_UL[-1] = -
. (IntegerType)count_I_LSB_DL[-1] = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 02 02 01 00

- No.: 1030
- Timestamp: 12:21:05:174_1
- RFN: 2283
- Chip: 20224
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 6
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 1031
- Timestamp: 12:21:05:174_2
- RFN: 2283
- Chip: 21760
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 7
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 3
. (IntegerType)count_I_LSB_UL[-1] = -
. (IntegerType)count_I_LSB_DL[-1] = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 03 02 01 00

- No.: 1032
- Timestamp: 12:21:05:175_0
- RFN: 2283
- Chip: 23296
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 8
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 3
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 1033
- Timestamp: 12:21:05:175_1
- RFN: 2283
- Chip: 24832
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 9
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 4
. (IntegerType)count_I_LSB_UL[-1] = -
. (IntegerType)count_I_LSB_DL[-1] = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 04 02 01 00

- No.: 1034
- Timestamp: 12:21:05:176_0
- RFN: 2283
- Chip: 26368
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 10
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 4
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 1038
- Timestamp: 12:21:05:177_0
- RFN: 2283
- Chip: 29696
- Event: Send
- PCO: CRLC
- Message: CRLC_Integrity_Activate_REQ
- Source: ts_CRLC_DL_Integrity LINE 1
- Message Structure:
CRLC_Integrity_Activate_REQ
. (IntegerType)cellId[-1] = -1
. (CN_DomainIdentity)cn_DomainIdentity[0] = 0
. IntegrityActivationInfo
. . IntegrityProtectionModeInfo
. . . IntegrityProtectionModeCommand
. . . . startIntegrityProtection
. . . . . (BitStringType)integrityProtInitNumber[32] = "00000000000000000000000000000001"
. . . (IntegrityProtectionAlgorithm)integrityProtectionAlgorithm[0] = 0
- Constraint:
ca_CRLC_DL_IntegrityActivateReq
- BinaryMessage:
30 14 02 01 ff 0a 01 00 30 0c 30 07 03 05 00 00 00 00 01 0a 01 00

- No.: 1039
- Timestamp: 12:21:05:177_1
- RFN: 2283
- Chip: 31488
- Event: Receive
- PCO: CRLC
- Message: CRLC_Integrity_Activate_CNF
- Source: ts_CRLC_DL_Integrity LINE 2
- Message Structure:
CRLC_Integrity_Activate_CNF
. (IntegerType)cellId[0] = -1
- Constraint:
ca_CRLC_IntegrityActivateCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1046
- Timestamp: 12:21:05:178_2
- RFN: 2283
- Chip: 36096
- Event: Send
- PCO: CRLC
- Message: CRLC_Integrity_Activate_REQ
- Source: ts_RB2_UL_IntegrityActivate LINE 1
- Message Structure:
CRLC_Integrity_Activate_REQ
. (IntegerType)cellId[-1] = -1
. (CN_DomainIdentity)cn_DomainIdentity[0] = 0
. IntegrityActivationInfo
. . IntegrityProtActivationInfoList
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity[-1] = 2
. . . . (IntegerType)rrc_MessageSequenceNumber[-1] = 0
- Constraint:
ca_CRLC_UL_IntegrityActivateReq
- BinaryMessage:
30 10 02 01 ff 0a 01 00 30 08 30 06 02 01 02 02 01 00

- No.: 1047
- Timestamp: 12:21:05:179_0
- RFN: 2283
- Chip: 37632
- Event: Receive
- PCO: CRLC
- Message: CRLC_Integrity_Activate_CNF
- Source: ts_RB2_UL_IntegrityActivate LINE 2
- Message Structure:
CRLC_Integrity_Activate_CNF
. (IntegerType)cellId[0] = -1
- Constraint:
ca_CRLC_IntegrityActivateCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1054
- Timestamp: 12:21:05:180_0
- RFN: 2284
- Chip: 4864
- Event: Send
- PCO: AM
- Message: RLC_AM_DATA_REQ
- Source: ts_RRC_Security:lt_SendSecurityModeCommand LINE 16
- Message Structure:
RLC_AM_DATA_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 2
. AmConfirmationRequest
. aM_message
. . DL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00000000000000000000000000000000"
. . . . (IntegerType)rrc_MessageSequenceNumber[-1] = 0
. . . DL_DCCH_MessageType
. . . . SecurityModeCommand
. . . . . r3
. . . . . . SecurityModeCommand_r3_IEs
. . . . . . . (IntegerType)rrc_TransactionIdentifier[-1] = 0
. . . . . . . SecurityCapability
. . . . . . . . (BitStringType)cipheringAlgorithmCap[16] = '0000000000000011'B
. . . . . . . . (BitStringType)integrityProtectionAlgorithmCap[16] = '0000000000000010'B
. . . . . . . CipheringModeInfo
. . . . . . . IntegrityProtectionModeInfo
. . . . . . . . IntegrityProtectionModeCommand
. . . . . . . . . startIntegrityProtection
. . . . . . . . . . (BitStringType)integrityProtInitNumber[32] = "00000000000000000000000000000001"
. . . . . . . . (IntegrityProtectionAlgorithm)integrityProtectionAlgorithm[0] = 0
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity[0] = 0
. . . . . . . InterRAT_UE_SecurityCapList
. . . . . . laterNonCriticalExtensions
- Constraint:
cas_RRC_SecModeCmd
- BinaryMessage:
30 17 02 01 ff 02 01 02 05 00 80 00 00 00 04 04 00 01 80 01 40 00 00 00 20

- No.: 1063
- Timestamp: 12:21:05:525_0
- RFN: 2318
- Chip: 24320
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_IND
- Source: ts_RRC_Security:lt_StartSecurity_UE LINE 8
- Message Structure:
RLC_AM_DATA_IND
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
. IntegrityResult
. . (IntegrityStatus)integrityUsed[0] = 0
. aM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "10000001100000001110110111011101"
. . . . (IntegerType)rrc_MessageSequenceNumber[4] = 1
. . . UL_DCCH_MessageType
. . . . SecurityModeComplete
. . . . . (IntegerType)rrc_TransactionIdentifier[2] = 0
. . . . . IntegrityProtActivationInfo
. . . . . . RRC_MessageSequenceNumberList
. . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . (IntegerType)_elem[4] = 0
. . . . . laterNonCriticalExtensions
- Constraint:
car_RRC_SecModeCmpl
- BinaryMessage:
30 12 02 01 ff 02 01 02 0a 01 00 c0 c0 76 ee 8d 21 00 00 00

- No.: 1064
- Timestamp: 12:21:05:525_1
- RFN: 2318
- Chip: 25856
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_Security:lt_StartSecurity_UE LINE 8
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1066
- Timestamp: 12:21:05:526_1
- RFN: 2318
- Chip: 28928
- Event: Send
- PCO: CRLC
- Message: CRLC_Integrity_Activate_REQ
- Source: ts_CRLC_UL_Integrity LINE 1
- Message Structure:
CRLC_Integrity_Activate_REQ
. (IntegerType)cellId[-1] = -1
. (CN_DomainIdentity)cn_DomainIdentity[0] = 0
. IntegrityActivationInfo
. . IntegrityProtActivationInfoList
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity[-1] = 0
. . . . (IntegerType)rrc_MessageSequenceNumber[-1] = 0
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity[-1] = 1
. . . . (IntegerType)rrc_MessageSequenceNumber[-1] = 0
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity[-1] = 3
. . . . (IntegerType)rrc_MessageSequenceNumber[-1] = 0
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity[-1] = 4
. . . . (IntegerType)rrc_MessageSequenceNumber[-1] = 0
- Constraint:
ca_CRLC_UL_IntegrityActivateReq
- BinaryMessage:
30 28 02 01 ff 0a 01 00 30 20 30 06 02 01 00 02 01 00 30 06 02 01 01 02 01 00 30 06 02 01 03 02 01 00 30 06 02 01 04 02 01 00

- No.: 1067
- Timestamp: 12:21:05:527_0
- RFN: 2318
- Chip: 30976
- Event: Receive
- PCO: CRLC
- Message: CRLC_Integrity_Activate_CNF
- Source: ts_CRLC_UL_Integrity LINE 2
- Message Structure:
CRLC_Integrity_Activate_CNF
. (IntegerType)cellId[0] = -1
- Constraint:
ca_CRLC_IntegrityActivateCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 1073
- Timestamp: 12:21:05:528_0
- RFN: 2318
- Chip: 36352
- Event: Send
- PCO: Dc
- Message: RRC_DataReq
- Source: ts_MM_IdleUpdated LINE 14
- Message Structure:
RRC_DataReq
. (IntegerType)cellId[-1] = -1
. (SS_RB_Identity)rB_Id[-1] = 3
. (LogicChGERAN)ch[-1] = -
. (SapId)sapId[1] = -
. (SS_CN_DomainIdentity)cN_Domain[-1] = 0
. LOCATIONUPDATINGACCEPT
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)mMProtocolDiscriminator[4] = '0101'B
. . (MsgType)msgType[8] = '00000010'B
. . LocAreaId_v
. . . (OctetStringType)plmn[3] = '00F110'O
. . . (OctetStringType)lac[2] = '0001'O
. . MM_MS_Identity
. . . (IEI8)iei[8] = '00010111'B
. . . (Length)iel[1] = '05'O
. . . (B4)iDigit1[4] = '1111'B
. . . (B1)oddEvenInd[1] = '0'B
. . . (B3)typeOfId[3] = '100'B
. . . (OctetStringType)otherDigits[-1] = '12345678'O
. . (FollowOnProceed)followOnProceed[8] = '10100001'B
. . (CTSPerm)cTSPerm[8] = '10100010'B
. . PLMN_List
. . . (IEI8)iei[8] = '01001010'B
. . . (Length)iel[1] = '03'O
. . . (OctetStringType)plmn1[3] = '00F312'O
. . . (OctetStringType)plmn2[3] = -
. . . (OctetStringType)plmn3[3] = -
. . . (OctetStringType)plmn4[3] = -
. . . (OctetStringType)plmn5[3] = -
- Constraint:
ca_DataReq
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 00 05 02 00 f1 10 00 01 17 05 f4 12 34 56 78 a1 a2 4a 03 00 f3 12

- No.: 1080
- Timestamp: 12:21:05:943_0
- RFN: 2360
- Chip: 19200
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_MM_IdleUpdated LINE 15
- Message Structure:
RRC_DataInd
. (IntegerType)cellId[0] = -1
. (SS_RB_Identity)rB_Id[0] = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain[0] = 0
. (START_Value)start[0] = -
. TMSIREALLOCATIONCOMPLETE
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)mMProtocolDiscriminator[4] = '0101'B
. . (MsgType)msgType[8] = '10011011'B
- Constraint:
car_UplinkDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 00 05 9b

- No.: 1091
- Timestamp: 12:21:05:945_2
- RFN: 2360
- Chip: 25088
- Event: Start Timer
- Source: ts_RRC_Delay LINE 1
- Message Structure:
no details available
- Constraint:
t_Dly (1000 Ms)
- BinaryMessage:

- No.: 1095
- Timestamp: 12:21:06:942_0
- RFN: 2460
- Chip: 12544
- Event: Timeout
- Source: ts_RRC_Delay LINE 2
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 1099
- Timestamp: 12:21:06:943_1
- RFN: 2460
- Chip: 16640
- Event: Send
- PCO: UM
- Message: RLC_UM_DATA_REQ
- Source: ts_RRC_ConnRel:lt_Send_RRC_ConnectionRelease LINE 7
- Message Structure:
RLC_UM_DATA_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 1
. uM_message
. . DL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00000000000000000000000000000000"
. . . . (IntegerType)rrc_MessageSequenceNumber[-1] = 0
. . . DL_DCCH_MessageType
. . . . RRCConnectionRelease
. . . . . r3
. . . . . . RRCConnectionRelease_r3_IEs
. . . . . . . (IntegerType)rrc_TransactionIdentifier[-1] = 0
. . . . . . . (IntegerType)n_308[-1] = -
. . . . . . . (ReleaseCause)releaseCause[0] = 0
. . . . . . . Rplmn_Information
. . . . . . laterNonCriticalExtensions
. (BooleanType)specialLI = FALSE
- Constraint:
cas_RRC_ConnRelDCCH
- BinaryMessage:
30 10 02 01 ff 02 01 01 80 00 00 00 03 c0 00 01 01 00

- No.: 1103
- Timestamp: 12:21:07:187_0
- RFN: 2484
- Chip: 33024
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_IND
- Source: ts_RRC_ConnRel:lt_Send_RRC_ConnectionRelease LINE 8
- Message Structure:
RLC_AM_DATA_IND
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
. IntegrityResult
. . (IntegrityStatus)integrityUsed[0] = 0
. aM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "01000011000100000000100001101011"
. . . . (IntegerType)rrc_MessageSequenceNumber[4] = 2
. . . UL_DCCH_MessageType
. . . . RRCConnectionReleaseComplete
. . . . . (IntegerType)rrc_TransactionIdentifier[2] = 0
. . . . . FailureCauseWithProtErr
. . . . . laterNonCriticalExtensions
- Constraint:
car_RRC_ConnRelCmpl
- BinaryMessage:
30 0f 02 01 ff 02 01 02 0a 01 00 a1 88 04 35 94 40

- No.: 1104
- Timestamp: 12:21:07:187_1
- RFN: 2484
- Chip: 34304
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ConnRel:lt_Send_RRC_ConnectionRelease LINE 8
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 1107
- Timestamp: 12:21:07:188_0
- RFN: 2484
- Chip: 36096
- Event: Start Timer
- Source: ts_RRC_Delay LINE 1
- Message Structure:
no details available
- Constraint:
t_Dly (1000 Ms)
- BinaryMessage:

- No.: 1111
- Timestamp: 12:21:08:190_0
- RFN: 2585
- Chip: 5120
- Event: Timeout
- Source: ts_RRC_Delay LINE 2
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 1118
- Timestamp: 12:21:08:192_0
- RFN: 2585
- Chip: 11264
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 1
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 01 0a 01 00 05 00

- No.: 1122
- Timestamp: 12:21:08:195_0
- RFN: 2585
- Chip: 22784
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 1125
- Timestamp: 12:21:08:196_0
- RFN: 2585
- Chip: 26624
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 2
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 02 0a 01 00 05 00

- No.: 1129
- Timestamp: 12:21:08:203_0
- RFN: 2586
- Chip: 15360
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 1132
- Timestamp: 12:21:08:204_0
- RFN: 2586
- Chip: 18176
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 3
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 03 0a 01 00 05 00

- No.: 1136
- Timestamp: 12:21:08:207_0
- RFN: 2586
- Chip: 32256
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 3
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 1139
- Timestamp: 12:21:08:208_0
- RFN: 2586
- Chip: 35328
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 4
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 04 0a 01 00 05 00

- No.: 1143
- Timestamp: 12:21:08:215_0
- RFN: 2587
- Chip: 22272
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 4
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 1146
- Timestamp: 12:21:08:216_0
- RFN: 2587
- Chip: 27648
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 1
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 136
. . . . . UL_RLC_Mode
. . . . . . UL_UM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (NoExplicitDiscard)timerBasedNoExplicit[0] = 9
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 1
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 1
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_UM_Info
- BinaryMessage:
30 22 02 01 ff 02 01 01 0a 01 00 30 17 30 0d 05 00 30 09 02 02 00 88 30 03 0a 01 09 30 06 02 01 01 02 01 01

- No.: 1150
- Timestamp: 12:21:08:224_0
- RFN: 2588
- Chip: 18432
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 1151
- Timestamp: 12:21:08:225_0
- RFN: 2588
- Chip: 24832
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 3
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 2
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 2
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 2
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 02 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 13 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 02 02 01 02

- No.: 1155
- Timestamp: 12:21:08:235_0
- RFN: 2589
- Chip: 24064
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 4
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 1156
- Timestamp: 12:21:08:236_0
- RFN: 2589
- Chip: 29696
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 5
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 3
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 3
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 3
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 03 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 13 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 03 02 01 03

- No.: 1160
- Timestamp: 12:21:08:247_0
- RFN: 2590
- Chip: 33280
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 6
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 3
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 1161
- Timestamp: 12:21:08:249_0
- RFN: 2591
- Chip: 512
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 7
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 4
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 4
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 4
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 04 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 13 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 04 02 01 04

- No.: 1165
- Timestamp: 12:21:08:259_0
- RFN: 2592
- Chip: 1024
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 8
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 4
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 1228
- Timestamp: 12:21:08:267_0
- RFN: 2592
- Chip: 30720
- Event: Send
- PCO: CPHY
- Message: CPHY_Cell_Config_REQ
- Source: ts_SS_CellCfg LINE 6
- Message Structure:
CPHY_Cell_Config_REQ
. (IntegerType)cellId[-1] = 3
. (IntegerType)tcell[-1] = 321
. (IntegerType)sfnOffset[-1] = 0
. FrequencyInfo
. . modeSpecificInfo
. . . FrequencyInfoFDD
. . . . (IntegerType)uarfcn_UL[-1] = 9663
. . . . (IntegerType)uarfcn_DL[-1] = 10613
. (IntegerType)primaryScramblingCode_SS[-1] = 200
. CellTxPowerLevel
. (IntegerType)dLTxAttenuationLevel[-1] = 2
- Constraint:
ca_CellCfgReq
- BinaryMessage:
30 1f 02 01 03 02 02 01 41 02 01 00 30 0a 30 08 02 02 25 bf 02 02 29 75 02 02 00 c8 05 00 02 01 02

- No.: 1232
- Timestamp: 12:21:08:633_0
- RFN: 2629
- Chip: 17920
- Event: Receive
- PCO: CPHY
- Message: CPHY_Cell_Config_CNF
- Source: ts_SS_CellCfg LINE 7
- Message Structure:
CPHY_Cell_Config_CNF
. (IntegerType)cellId[0] = 3
- Constraint:
ca_CellCfgCnf
- BinaryMessage:
30 03 02 01 03

- No.: 1244
- Timestamp: 12:21:08:635_0
- RFN: 2629
- Chip: 25856
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 3
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 0
. (RatType)ratType[0] = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . PrimaryCPICHInfo
. . . . (IntegerType)dl_TxPower_PCPICH[-1] = -60
. . . . (BooleanType)txdiversityIndicator = FALSE
- Constraint:
ca_pCPICH_Info
- BinaryMessage:
30 13 02 01 03 02 01 00 0a 01 00 30 08 30 06 02 01 c4 01 01 00

- No.: 1248
- Timestamp: 12:21:08:639_0
- RFN: 2630
- Chip: 3584
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 4
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId[0] = 3
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 0
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 03 02 01 00

- No.: 1249
- Timestamp: 12:21:08:640_0
- RFN: 2630
- Chip: 5888
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 5
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 1
. (RatType)ratType[0] = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . PrimarySCHInfo
. . . . (BooleanType)tstdIndicator = FALSE
. . . . (IntegerType)dl_TxPower[-1] = -5
- Constraint:
ca_pSCH_Info
- BinaryMessage:
30 13 02 01 03 02 01 01 0a 01 00 30 08 30 06 01 01 00 02 01 fb

- No.: 1253
- Timestamp: 12:21:08:643_0
- RFN: 2630
- Chip: 18176
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 6
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId[0] = 3
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 1
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 03 02 01 01

- No.: 1254
- Timestamp: 12:21:08:644_0
- RFN: 2630
- Chip: 20736
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 7
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 2
. (RatType)ratType[0] = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . SecondarySCHInfo
. . . . (BooleanType)tstdIndicator = FALSE
. . . . (IntegerType)dl_TxPower[-1] = -5
- Constraint:
ca_sSCH_Info
- BinaryMessage:
30 13 02 01 03 02 01 02 0a 01 00 30 08 30 06 01 01 00 02 01 fb

- No.: 1258
- Timestamp: 12:21:08:782_0
- RFN: 2644
- Chip: 15872
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 8
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId[0] = 3
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 2
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 03 02 01 02

- No.: 1259
- Timestamp: 12:21:08:783_0
- RFN: 2644
- Chip: 18432
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 9
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 4
. (RatType)ratType[0] = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . PrimaryCCPCHInfo
. . . . (BooleanType)sttd_Indicator = FALSE
. . . . (IntegerType)dl_TxPower[-1] = -2
- Constraint:
ca_pCCPCH_Info
- BinaryMessage:
30 13 02 01 03 02 01 04 0a 01 00 30 08 30 06 01 01 00 02 01 fe

- No.: 1263
- Timestamp: 12:21:08:790_0
- RFN: 2645
- Chip: 8192
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 10
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId[0] = 3
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 4
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 03 02 01 04

- No.: 1264
- Timestamp: 12:21:08:792_0
- RFN: 2645
- Chip: 16384
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Config_REQ
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 11
- Message Structure:
CPHY_TrCH_Config_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 4
. (RatType)ratType[0] = 0
. TrChConfigType
. CphyTrchConfigReq
. . SS_ActivationTime
. . ulconnectedTrCHList
. . TFCS
. . dlconnectedTrCHList
. . . CphyTrchConfigReq_setseq_1
. . . . (IntegerType)trchid[-1] = 11
. . . . (SS_DL_TransportChannelType)dl_TransportChannelType[0] = 2
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size[-1] = 246
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional[0] = 0
. . . . . . (IntegerType)rateMatchingAttribute[-1] = 1
. . . . . . (CRC_Size)crc_Size[0] = 3
. . TFCS
. . . ExplicitTFCS_Configuration
. . . . TFCS_ReconfAdd
. . . . . ctfcSize
. . . . . . ctfc2Bit
. . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . (IntegerType)ctfc2[-1] = 0
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . fdd
. . . . . . . . . . . . . (IntegerType)gainFactorBetaC[-1] = 11
. . . . . . . . . . . (IntegerType)gainFactorBetaD[-1] = 15
. . . . . . . . . . . (IntegerType)referenceTFC_ID[-1] = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
- Constraint:
ca_BCH_InfoActNow
- BinaryMessage:
30 4c 02 01 03 02 01 04 0a 01 00 05 00 30 3f 05 00 30 23 30 21 02 01 0b 0a 01 02 30 19 30 0c 30 0a 02 02 00 f6 30 02 05 00 05 00 30 09 0a 01 00 02 01 01 0a 01 03 30 16 30 14 30 12 02 01 00 30 0d 30 0b 30 03 02 01 0b 02 01 0f 02 01 00

- No.: 1268
- Timestamp: 12:21:08:800_0
- RFN: 2646
- Chip: 2816
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Config_CNF
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 12
- Message Structure:
CPHY_TrCH_Config_CNF
. (IntegerType)cellId[0] = 3
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 4
- Constraint:
ca_TrChCfgCnf
- BinaryMessage:
30 06 02 01 03 02 01 04

- No.: 1269
- Timestamp: 12:21:08:803_0
- RFN: 2646
- Chip: 17408
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 13
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 4
. (RatType)ratType[0] = 0
. configMessage
. . CmacConfigReq
. . . SS_ActivationTime
. . . UE_Info
. . . . U_RNTI
. . . . (BitStringType)c_RNTI[16] = -
. . . TrCHInfo
. . . . ulconnectedTrCHList
. . . . TFCS
. . . . dlconnectedTrCHList
. . . . . TrCHInfo_setseq_1
. . . . . . (IntegerType)trchid[-1] = 11
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size[-1] = 246
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional[0] = 0
. . . . . . . . (IntegerType)rateMatchingAttribute[-1] = 1
. . . . . . . . (CRC_Size)crc_Size[0] = 3
. . . . TFCS
. . . . . ExplicitTFCS_Configuration
. . . . . . TFCS_ReconfAdd
. . . . . . . ctfcSize
. . . . . . . . ctfc2Bit
. . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . (IntegerType)ctfc2[-1] = 0
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC[-1] = 11
. . . . . . . . . . . . . (IntegerType)gainFactorBetaD[-1] = 15
. . . . . . . . . . . . . (IntegerType)referenceTFC_ID[-1] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . TrCH_LogCHMappingList1
. . . . ulconnectedTrCHList
. . . . dlconnectedTrCHList
. . . . . TrCH_LogCHMappingList1_setseq_1
. . . . . . (IntegerType)trchid[-1] = 11
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation[0] = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType[0] = 2
. . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . . . (LogicalChannelType)logicalChannelType[0] = 0
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 1
. . . . . . . . (IntegerType)rB_Identity[-1] = -1
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_CMAC_CfgInfo
- BinaryMessage:
30 6e 02 01 03 02 01 04 0a 01 00 30 63 05 00 30 00 30 3a 30 20 30 1e 02 01 0b 30 19 30 0c 30 0a 02 02 00 f6 30 02 05 00 05 00 30 09 0a 01 00 02 01 01 0a 01 03 30 16 30 14 30 12 02 01 00 30 0d 30 0b 30 03 02 01 0b 02 01 0f 02 01 00 30 21 30 1f 30 1d 02 01 0b 30 18 30 16 30 11 0a 01 00 0a 01 02 02 01 01 0a 01 00 05 00 02 01 01 02 01 ff

- No.: 1273
- Timestamp: 12:21:08:808_0
- RFN: 2646
- Chip: 36864
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 14
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId[0] = 3
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 4
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 03 02 01 04

- No.: 1310
- Timestamp: 12:21:08:813_0
- RFN: 2647
- Chip: 17152
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_PCH_FACH_CCCH_Cfg LINE 3
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 5
. (RatType)ratType[0] = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . SecondaryCCPCHInfo
. . . . (IntegerType)scramblingCode[-1] = 0
. . . . SF256_AndCodeNumber
. . . . . (IntegerType)sf64[-1] = 1
. . . . (IntegerType)sCCPCHSlotFormat[-1] = 8
. . . . (IntegerType)timingOffset[-1] = 0
. . . . (PositionFixedOrFlexible)positionFixedOrFlexible[0] = 1
. . . . (BooleanType)sttd_Indicator = FALSE
. . . . (IntegerType)dl_TxPower[-1] = -2
. . . . (IntegerType)powerOffsetOfTFCI_PO1[-1] = 6
. . . . (IntegerType)powerOffsetOfPILOT_PO3[-1] = 6
- Constraint:
ca_sCCPCH_Info
- BinaryMessage:
30 28 02 01 03 02 01 05 0a 01 00 30 1d 30 1b 02 01 00 02 01 01 02 01 08 02 01 00 0a 01 01 01 01 00 02 01 fe 02 01 06 02 01 06

- No.: 1314
- Timestamp: 12:21:08:818_0
- RFN: 2647
- Chip: 34304
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_PCH_FACH_CCCH_Cfg LINE 4
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId[0] = 3
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 5
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 03 02 01 05

- No.: 1315
- Timestamp: 12:21:08:826_0
- RFN: 2648
- Chip: 27392
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Config_REQ
- Source: ts_SS_PCH_FACH_CCCH_Cfg LINE 5
- Message Structure:
CPHY_TrCH_Config_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 5
. (RatType)ratType[0] = 0
. TrChConfigType
. CphyTrchConfigReq
. . SS_ActivationTime
. . ulconnectedTrCHList
. . TFCS
. . dlconnectedTrCHList
. . . CphyTrchConfigReq_setseq_1
. . . . (IntegerType)trchid[-1] = 12
. . . . (SS_DL_TransportChannelType)dl_TransportChannelType[0] = 3
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size[-1] = 240
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional[0] = 0
. . . . . . (IntegerType)rateMatchingAttribute[-1] = 230
. . . . . . (CRC_Size)crc_Size[0] = 3
. . . CphyTrchConfigReq_setseq_1
. . . . (IntegerType)trchid[-1] = 13
. . . . (SS_DL_TransportChannelType)dl_TransportChannelType[0] = 1
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size[-1] = 168
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . (IntegerType)small[-1] = 2
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional[0] = 0
. . . . . . (IntegerType)rateMatchingAttribute[-1] = 220
. . . . . . (CRC_Size)crc_Size[0] = 3
. . . CphyTrchConfigReq_setseq_1
. . . . (IntegerType)trchid[-1] = 14
. . . . (SS_DL_TransportChannelType)dl_TransportChannelType[0] = 1
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size[-1] = 360
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . (IntegerType)rateMatchingAttribute[-1] = 130
. . . . . . (CRC_Size)crc_Size[0] = 3
. . TFCS
. . . ExplicitTFCS_Configuration
. . . . TFCS_ReconfAdd
. . . . . ctfcSize
. . . . . . ctfc4Bit
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4[-1] = 0
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4[-1] = 1
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4[-1] = 2
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4[-1] = 3
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4[-1] = 4
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4[-1] = 5
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4[-1] = 6
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4[-1] = 8
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . fdd
. . . . . . . . . . . . . (IntegerType)gainFactorBetaC[-1] = 11
. . . . . . . . . . . (IntegerType)gainFactorBetaD[-1] = 15
. . . . . . . . . . . (IntegerType)referenceTFC_ID[-1] = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
- Constraint:
ca_PCH_2_FACH_InfoActNow
- BinaryMessage:
30 81 e4 02 01 03 02 01 05 0a 01 00 05 00 30 81 d6 05 00 30 74 30 24 02 01 0c 0a 01 03 30 1c 30 0e 30 0c 02 02 00 f0 30 04 05 00 05 00 05 00 30 0a 0a 01 00 02 02 00 e6 0a 01 03 30 27 02 01 0d 0a 01 01 30 1f 30 11 30 0f 02 02 00 a8 30 07 05 00 05 00 02 01 02 05 00 30 0a 0a 01 00 02 02 00 dc 0a 01 03 30 23 02 01 0e 0a 01 01 30 1b 30 0e 30 0c 02 02 01 68 30 04 05 00 05 00 05 00 30 09 05 00 02 02 00 82 0a 01 03 30 5c 30 5a 30 08 02 01 00 30 03 02 01 00 30 08 02 01 01 30 03 02 01 00 30 08 02 01 02 30 03 02 01 00 30 08 02 01 03 30 03 02 01 00 30 08 02 01 04 30 03 02 01 00 30 08 02 01 05 30 03 02 01 00 30 08 02 01 06 30 03 02 01 00 30 12 02 01 08 30 0d 30 0b 30 03 02 01 0b 02 01 0f 02 01 00

- No.: 1319
- Timestamp: 12:21:08:834_0
- RFN: 2649
- Chip: 21504
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Config_CNF
- Source: ts_SS_PCH_FACH_CCCH_Cfg LINE 6
- Message Structure:
CPHY_TrCH_Config_CNF
. (IntegerType)cellId[0] = 3
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 5
- Constraint:
ca_TrChCfgCnf
- BinaryMessage:
30 06 02 01 03 02 01 05

- No.: 1320
- Timestamp: 12:21:08:844_0
- RFN: 2650
- Chip: 19456
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_SS_PCH_FACH_CCCH_Cfg LINE 7
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 5
. (RatType)ratType[0] = 0
. configMessage
. . CmacConfigReq
. . . SS_ActivationTime
. . . UE_Info
. . . . U_RNTI
. . . . (BitStringType)c_RNTI[16] = -
. . . TrCHInfo
. . . . ulconnectedTrCHList
. . . . TFCS
. . . . dlconnectedTrCHList
. . . . . TrCHInfo_setseq_1
. . . . . . (IntegerType)trchid[-1] = 12
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size[-1] = 240
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional[0] = 0
. . . . . . . . (IntegerType)rateMatchingAttribute[-1] = 230
. . . . . . . . (CRC_Size)crc_Size[0] = 3
. . . . . TrCHInfo_setseq_1
. . . . . . (IntegerType)trchid[-1] = 13
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size[-1] = 168
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . (IntegerType)small[-1] = 2
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional[0] = 0
. . . . . . . . (IntegerType)rateMatchingAttribute[-1] = 220
. . . . . . . . (CRC_Size)crc_Size[0] = 3
. . . . . TrCHInfo_setseq_1
. . . . . . (IntegerType)trchid[-1] = 14
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size[-1] = 360
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . (IntegerType)rateMatchingAttribute[-1] = 130
. . . . . . . . (CRC_Size)crc_Size[0] = 3
. . . . TFCS
. . . . . ExplicitTFCS_Configuration
. . . . . . TFCS_ReconfAdd
. . . . . . . ctfcSize
. . . . . . . . ctfc4Bit
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4[-1] = 0
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4[-1] = 1
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4[-1] = 2
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4[-1] = 3
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4[-1] = 4
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4[-1] = 5
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4[-1] = 6
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4[-1] = 8
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC[-1] = 11
. . . . . . . . . . . . . (IntegerType)gainFactorBetaD[-1] = 15
. . . . . . . . . . . . . (IntegerType)referenceTFC_ID[-1] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . TrCH_LogCHMappingList1
. . . . ulconnectedTrCHList
. . . . dlconnectedTrCHList
. . . . . TrCH_LogCHMappingList1_setseq_1
. . . . . . (IntegerType)trchid[-1] = 12
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation[0] = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType[0] = 3
. . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . . . (LogicalChannelType)logicalChannelType[0] = 1
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 1
. . . . . . . . (IntegerType)rB_Identity[-1] = -2
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
. . . . . TrCH_LogCHMappingList1_setseq_1
. . . . . . (IntegerType)trchid[-1] = 13
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation[0] = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType[0] = 1
. . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 5
. . . . . . . . . . (LogicalChannelType)logicalChannelType[0] = 2
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 1
. . . . . . . . (IntegerType)rB_Identity[-1] = 0
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_CMAC_CfgInfo
- BinaryMessage:
30 82 01 21 02 01 03 02 01 05 0a 01 00 30 82 01 14 05 00 30 00 30 81 cb 30 6b 30 21 02 01 0c 30 1c 30 0e 30 0c 02 02 00 f0 30 04 05 00 05 00 05 00 30 0a 0a 01 00 02 02 00 e6 0a 01 03 30 24 02 01 0d 30 1f 30 11 30 0f 02 02 00 a8 30 07 05 00 05 00 02 01 02 05 00 30 0a 0a 01 00 02 02 00 dc 0a 01 03 30 20 02 01 0e 30 1b 30 0e 30 0c 02 02 01 68 30 04 05 00 05 00 05 00 30 09 05 00 02 02 00 82 0a 01 03 30 5c 30 5a 30 08 02 01 00 30 03 02 01 00 30 08 02 01 01 30 03 02 01 00 30 08 02 01 02 30 03 02 01 00 30 08 02 01 03 30 03 02 01 00 30 08 02 01 04 30 03 02 01 00 30 08 02 01 05 30 03 02 01 00 30 08 02 01 06 30 03 02 01 00 30 12 02 01 08 30 0d 30 0b 30 03 02 01 0b 02 01 0f 02 01 00 30 40 30 3e 30 1d 02 01 0c 30 18 30 16 30 11 0a 01 00 0a 01 03 02 01 01 0a 01 01 05 00 02 01 01 02 01 fe 30 1d 02 01 0d 30 18 30 16 30 11 0a 01 00 0a 01 01 02 01 05 0a 01 02 05 00 02 01 01 02 01 00

- No.: 1324
- Timestamp: 12:21:08:854_0
- RFN: 2651
- Chip: 21248
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_SS_PCH_FACH_CCCH_Cfg LINE 8
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId[0] = 3
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 5
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 03 02 01 05

- No.: 1325
- Timestamp: 12:21:08:855_0
- RFN: 2651
- Chip: 25088
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_PCH_FACH_CCCH_Cfg LINE 9
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 6
. (RatType)ratType[0] = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . PICHInfo
. . . . PICH_Info
. . . . . fdd
. . . . . . (IntegerType)channelisationCode256[-1] = 2
. . . . . . (PI_CountPerFrame)pi_CountPerFrame[0] = 0
. . . . . . (BooleanType)sttd_Indicator = FALSE
. . . . (IntegerType)dl_TxPower[-1] = -5
. . . . (IntegerType)sccpchId_associated[-1] = 5
- Constraint:
ca_PICH_Info
- BinaryMessage:
30 1e 02 01 03 02 01 06 0a 01 00 30 13 30 11 30 09 02 01 02 0a 01 00 01 01 00 02 01 fb 02 01 05

- No.: 1329
- Timestamp: 12:21:08:862_0
- RFN: 2652
- Chip: 13056
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_PCH_FACH_CCCH_Cfg LINE 10
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId[0] = 3
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 6
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 03 02 01 06

- No.: 1337
- Timestamp: 12:21:08:864_0
- RFN: 2652
- Chip: 19712
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_RACH_CCCH_Cfg LINE 3
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 7
. (RatType)ratType[0] = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . AICHInfo
. . . . AICH_Info
. . . . . (IntegerType)channelisationCode256[-1] = 3
. . . . . (BooleanType)sttd_Indicator = FALSE
. . . . . (AICH_TransmissionTiming)aich_TransmissionTiming[0] = 0
. . . . (IntegerType)dl_TxPower[-1] = -5
- Constraint:
ca_AichInfo
- BinaryMessage:
30 1b 02 01 03 02 01 07 0a 01 00 30 10 30 0e 30 09 02 01 03 01 01 00 0a 01 00 02 01 fb

- No.: 1341
- Timestamp: 12:21:08:869_0
- RFN: 2653
- Chip: 2560
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_RACH_CCCH_Cfg LINE 4
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId[0] = 3
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 7
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 03 02 01 07

- No.: 1342
- Timestamp: 12:21:08:870_0
- RFN: 2653
- Chip: 6144
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_RACH_CCCH_Cfg LINE 5
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 8
. (RatType)ratType[0] = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . PRACHInfo
. . . . fdd_tdd
. . . . . fdd
. . . . . . (BitStringType)preambleSignature[16] = "0000000011111111"
. . . . . . (SF_PRACH)spreadingFactorForDataPart[0] = 1
. . . . . . (IntegerType)preambleScramblingCode[-1] = 0
. . . . . . (PuncturingLimit)puncturingLimit[0] = 15
. . . . . . (BitStringType)accessSlot[12] = "111111111111"
- Constraint:
ca_PRACH_Info
- BinaryMessage:
30 22 02 01 03 02 01 08 0a 01 00 30 17 30 15 30 13 03 03 00 00 00 0a 01 01 02 01 00 0a 01 0f 03 03 04 ff ff

- No.: 1346
- Timestamp: 12:21:08:876_0
- RFN: 2653
- Chip: 26880
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_RACH_CCCH_Cfg LINE 6
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId[0] = 3
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 8
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 03 02 01 08

- No.: 1347
- Timestamp: 12:21:08:878_0
- RFN: 2653
- Chip: 35328
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Config_REQ
- Source: ts_SS_RACH_CCCH_Cfg LINE 7
- Message Structure:
CPHY_TrCH_Config_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 8
. (RatType)ratType[0] = 0
. TrChConfigType
. CphyTrchConfigReq
. . SS_ActivationTime
. . ulconnectedTrCHList
. . . CphyTrchConfigReq_setseq_0
. . . . (IntegerType)trchid[-1] = 15
. . . . (SS_UL_TransportChannelType)ul_TransportChannelType[0] = 1
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size[-1] = 168
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size[-1] = 360
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional[0] = 0
. . . . . . (IntegerType)rateMatchingAttribute[-1] = 150
. . . . . . (CRC_Size)crc_Size[0] = 3
. . TFCS
. . . ExplicitTFCS_Configuration
. . . . TFCS_ReconfAdd
. . . . . ctfcSize
. . . . . . ctfc2Bit
. . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . (IntegerType)ctfc2[-1] = 0
. . . . . . . . PowerOffsetInformation
. . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . (IntegerType)ctfc2[-1] = 1
. . . . . . . . PowerOffsetInformation
. . dlconnectedTrCHList
. . TFCS
- Constraint:
cab_RACH_InfoActNow
- BinaryMessage:
30 4f 02 01 03 02 01 08 0a 01 00 05 00 30 42 05 00 30 30 30 2e 02 01 0f 0a 01 01 30 26 30 18 30 0a 02 02 00 a8 30 02 05 00 05 00 30 0a 02 02 01 68 30 02 05 00 05 00 30 0a 0a 01 00 02 02 00 96 0a 01 03 30 0c 30 0a 30 03 02 01 00 30 03 02 01 01

- No.: 1351
- Timestamp: 12:21:08:889_0
- RFN: 2654
- Chip: 38144
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Config_CNF
- Source: ts_SS_RACH_CCCH_Cfg LINE 8
- Message Structure:
CPHY_TrCH_Config_CNF
. (IntegerType)cellId[0] = 3
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 8
- Constraint:
ca_TrChCfgCnf
- BinaryMessage:
30 06 02 01 03 02 01 08

- No.: 1352
- Timestamp: 12:21:08:892_0
- RFN: 2655
- Chip: 13824
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_SS_RACH_CCCH_Cfg LINE 9
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 8
. (RatType)ratType[0] = 0
. configMessage
. . CmacConfigReq
. . . SS_ActivationTime
. . . UE_Info
. . . . U_RNTI
. . . . (BitStringType)c_RNTI[16] = -
. . . TrCHInfo
. . . . ulconnectedTrCHList
. . . . . TrCHInfo_setseq_0
. . . . . . (IntegerType)trchid[-1] = 15
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size[-1] = 168
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size[-1] = 360
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional[0] = 0
. . . . . . . . (IntegerType)rateMatchingAttribute[-1] = 150
. . . . . . . . (CRC_Size)crc_Size[0] = 3
. . . . TFCS
. . . . . ExplicitTFCS_Configuration
. . . . . . TFCS_ReconfAdd
. . . . . . . ctfcSize
. . . . . . . . ctfc2Bit
. . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . (IntegerType)ctfc2[-1] = 0
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . (IntegerType)ctfc2[-1] = 1
. . . . . . . . . . PowerOffsetInformation
. . . . dlconnectedTrCHList
. . . . TFCS
. . . TrCH_LogCHMappingList1
. . . . ulconnectedTrCHList
. . . . . TrCH_LogCHMappingList1_setseq_0
. . . . . . (IntegerType)trchid[-1] = 15
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation[0] = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType[0] = 1
. . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 5
. . . . . . . . . . (LogicalChannelType)logicalChannelType[0] = 2
. . . . . . . . (IntegerType)rB_Identity[-1] = 0
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
. . . . dlconnectedTrCHList
- Constraint:
ca_CMAC_CfgInfo
- BinaryMessage:
30 6c 02 01 03 02 01 08 0a 01 00 30 61 05 00 30 00 30 3d 30 2d 30 2b 02 01 0f 30 26 30 18 30 0a 02 02 00 a8 30 02 05 00 05 00 30 0a 02 02 01 68 30 02 05 00 05 00 30 0a 0a 01 00 02 02 00 96 0a 01 03 30 0c 30 0a 30 03 02 01 00 30 03 02 01 01 30 1c 30 1a 30 18 02 01 0f 30 13 30 11 30 0c 0a 01 00 0a 01 01 02 01 05 0a 01 02 02 01 00

- No.: 1356
- Timestamp: 12:21:08:897_0
- RFN: 2655
- Chip: 32256
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_SS_RACH_CCCH_Cfg LINE 10
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId[0] = 3
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 8
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 03 02 01 08

- No.: 1359
- Timestamp: 12:21:08:898_0
- RFN: 2655
- Chip: 37632
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB_BCCH_BCH_Cfg LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 246
. . . . . UL_RLC_Mode
. . . . . . UL_TM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . (BooleanType)segmentationIndication = FALSE
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[0] = -
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 1
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_BCCH_Info
- BinaryMessage:
30 1d 02 01 03 02 01 ff 0a 01 00 30 12 30 0b 30 09 02 02 00 f6 30 03 01 01 00 30 03 02 01 01

- No.: 1363
- Timestamp: 12:21:08:902_0
- RFN: 2656
- Chip: 14848
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB_BCCH_BCH_Cfg LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 03 02 01 ff

- No.: 1366
- Timestamp: 12:21:08:904_0
- RFN: 2656
- Chip: 20736
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB_PCCH_Cfg LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -2
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 240
. . . . . UL_RLC_Mode
. . . . . . UL_TM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . (BooleanType)segmentationIndication = FALSE
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[0] = -
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 1
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_PCCH_Info
- BinaryMessage:
30 1d 02 01 03 02 01 fe 0a 01 00 30 12 30 0b 30 09 02 02 00 f0 30 03 01 01 00 30 03 02 01 01

- No.: 1370
- Timestamp: 12:21:08:906_0
- RFN: 2656
- Chip: 29184
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB_PCCH_Cfg LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 03 02 01 fe

- No.: 1373
- Timestamp: 12:21:08:908_0
- RFN: 2656
- Chip: 35584
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB0_Cfg LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 0
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 152
. . . . . UL_RLC_Mode
. . . . . . UL_UM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (NoExplicitDiscard)timerBasedNoExplicit[0] = 9
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[0] = -
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 5
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_UM_DL_Info
- BinaryMessage:
30 1d 02 01 03 02 01 00 0a 01 00 30 12 30 0b 30 09 02 02 00 98 30 03 0a 01 09 30 03 02 01 05

- No.: 1377
- Timestamp: 12:21:08:913_0
- RFN: 2657
- Chip: 16128
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB0_Cfg LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 0
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 03 02 01 00

- No.: 1378
- Timestamp: 12:21:08:914_0
- RFN: 2657
- Chip: 21504
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB0_Cfg LINE 3
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 0
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_TM_RLC_Mode
. . . . . . (BooleanType)segmentationIndication = FALSE
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 166
. . . . . UL_RLC_Mode
. . . . . . UL_TM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . (BooleanType)segmentationIndication = FALSE
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 5
. . . . (IntegerType)dLlogicalChannelIdentity[0] = -
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_TM_UL_Info
- BinaryMessage:
30 22 02 01 03 02 01 00 0a 01 00 30 17 30 10 30 03 01 01 00 30 09 02 02 00 a6 30 03 01 01 00 30 03 02 01 05

- No.: 1382
- Timestamp: 12:21:08:919_0
- RFN: 2658
- Chip: 512
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB0_Cfg LINE 4
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 0
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 03 02 01 00

- No.: 1444
- Timestamp: 12:21:08:936_0
- RFN: 2659
- Chip: 29440
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 10
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 03 02 01 ff 0a 01 00 30 06 02 01 06 02 01 0a

- No.: 1449
- Timestamp: 12:21:08:938_0
- RFN: 2659
- Chip: 37120
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB1_LongNeighCellInfo LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 03 02 01 ff

- No.: 1450
- Timestamp: 12:21:08:939_0
- RFN: 2660
- Chip: 1536
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB1_LongNeighCellInfo LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 1
. . . . . . . (BitStringType)sib_Data_variable[-1] = "1100010000000000000001011000100000001000000000100001000111100000000101111111111111111111111110100101100011011011100110111111111010010101011101010011101001110111111001111010011"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 2
. . . . . . . (BitStringType)sib_Data_variable[-1] = "00000000000000000010"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 24 02 01 03 02 01 ff 00 0e 21 ae c4 00 05 88 08 02 11 e0 17 ff ff fa 58 db 9b fe 95 75 3a 77 e7 a6 21 30 00 02

- No.: 1463
- Timestamp: 12:21:08:943_0
- RFN: 2660
- Chip: 16384
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 10
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 03 02 01 ff 0a 01 00 30 06 02 01 06 02 01 0a

- No.: 1468
- Timestamp: 12:21:08:952_0
- RFN: 2661
- Chip: 13568
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB2_LongNeighCellInfo LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 03 02 01 ff

- No.: 1469
- Timestamp: 12:21:08:953_0
- RFN: 2661
- Chip: 16896
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB2_LongNeighCellInfo LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 1
. . . . . . . (BitStringType)sib_Data_variable[-1] = "1100010000000000000001011000100000001000000000100001000111100000000101111111111111111111111110100101100011011011100110111111111010010101011101010011101001110111111001111010011"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 2
. . . . . . . (BitStringType)sib_Data_variable[-1] = "00000000000000000010"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 24 02 01 03 02 01 ff 00 0e 21 ae c4 00 05 88 08 02 11 e0 17 ff ff fa 58 db 9b fe 95 75 3a 77 e7 a6 21 30 00 02

- No.: 1481
- Timestamp: 12:21:08:956_1
- RFN: 2661
- Chip: 29440
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 7
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 03 02 01 ff 0a 01 00 30 06 02 01 06 02 01 07

- No.: 1486
- Timestamp: 12:21:08:962_0
- RFN: 2662
- Chip: 13824
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB3_LongNeighCellInfo LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 03 02 01 ff

- No.: 1487
- Timestamp: 12:21:08:963_0
- RFN: 2662
- Chip: 16640
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB3_LongNeighCellInfo LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 7
. . . . . . . (BitStringType)sib_Data_variable[-1] = "100000101000000010000001"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 3
. . . . . . . (BitStringType)sib_Data_variable[-1] = "010000000000000000000000000011001011001100011000010000000000001000000100011111111111111111111111"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 1b 02 01 03 02 01 ff 00 0e 27 17 82 80 81 1a fa 00 00 00 65 98 c2 00 10 23 ff ff f8

- No.: 1499
- Timestamp: 12:21:08:966_0
- RFN: 2662
- Chip: 29696
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 31
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 03 02 01 ff 0a 01 00 30 06 02 01 06 02 01 1f

- No.: 1504
- Timestamp: 12:21:08:972_0
- RFN: 2663
- Chip: 12544
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB4_LongNeighCellInfo LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 03 02 01 ff

- No.: 1505
- Timestamp: 12:21:08:972_1
- RFN: 2663
- Chip: 15360
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB4_LongNeighCellInfo LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 7
. . . . . . . (BitStringType)sib_Data_variable[-1] = "100000101000000010000001"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 4
. . . . . . . (BitStringType)sib_Data_variable[-1] = "0000000000000000000000000001100101100110001100001000000000000100000010001110111"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 19 02 01 03 02 01 ff 00 0e 27 17 82 80 81 22 70 00 00 00 cb 31 84 00 20 47 70

- No.: 1522
- Timestamp: 12:21:08:982_0
- RFN: 2664
- Chip: 13824
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 22
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 03 02 01 ff 0a 01 00 30 06 02 01 06 02 01 16

- No.: 1527
- Timestamp: 12:21:08:991_0
- RFN: 2665
- Chip: 12544
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB5_LongNeighCellInfo LINE 41
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 03 02 01 ff

- No.: 1528
- Timestamp: 12:21:08:992_0
- RFN: 2665
- Chip: 14848
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB5_LongNeighCellInfo LINE 42
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 08 02 01 03 02 01 ff 00 00

- No.: 1532
- Timestamp: 12:21:08:993_1
- RFN: 2665
- Chip: 18432
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 18
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 03 02 01 ff 0a 01 00 30 06 02 01 06 02 01 12

- No.: 1537
- Timestamp: 12:21:09:002_0
- RFN: 2666
- Chip: 13568
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB5_LongNeighCellInfo LINE 44
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 03 02 01 ff

- No.: 1538
- Timestamp: 12:21:09:003_0
- RFN: 2666
- Chip: 17152
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB5_LongNeighCellInfo LINE 45
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . FirstSegment
. . . . . . (SIB_Type)sib_Type[0] = 5
. . . . . . (IntegerType)seg_Count[-1] = 3
. . . . . . (BitStringType)sib_Data_fixed[222] = "000101010100010000111110000000001111111101000011111111111111110111010010000100001111000000101001000011000000101010100101010110000000000000001100110001011011010101111110001010111010000011111110100000111111101000001111111010"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 25 02 01 03 02 01 ff 00 02 52 15 44 3e 00 ff 43 ff fd d2 10 f0 29 0c 0a a5 58 00 0c c5 b5 7e 2b a0 fe 83 fa 0f e8

- No.: 1542
- Timestamp: 12:21:09:004_0
- RFN: 2666
- Chip: 23808
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 19
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 03 02 01 ff 0a 01 00 30 06 02 01 06 02 01 13

- No.: 1547
- Timestamp: 12:21:09:012_0
- RFN: 2667
- Chip: 13312
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB5_LongNeighCellInfo LINE 47
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 03 02 01 ff

- No.: 1548
- Timestamp: 12:21:09:012_1
- RFN: 2667
- Chip: 15872
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB5_LongNeighCellInfo LINE 48
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . SubsequentSegment
. . . . . . (SIB_Type)sib_Type[0] = 5
. . . . . . (IntegerType)segmentIndex[-1] = 1
. . . . . . (BitStringType)sib_Data_fixed[222] = "000011111111010000000000000000001101011000110100010000111111010011100101000001100001000011001010000000110000001110001001000000010110000000000000100000001110000000001000100001100100001010011001000010100000000000110000000100"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 25 02 01 03 02 01 ff 00 04 50 0f f4 00 00 d6 34 43 f4 e5 06 10 ca 03 03 89 01 60 00 80 e0 08 86 42 99 0a 00 30 10

- No.: 1552
- Timestamp: 12:21:09:013_3
- RFN: 2667
- Chip: 19712
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 21
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 03 02 01 ff 0a 01 00 30 06 02 01 06 02 01 15

- No.: 1557
- Timestamp: 12:21:09:022_0
- RFN: 2668
- Chip: 13056
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB5_LongNeighCellInfo LINE 50
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 03 02 01 ff

- No.: 1559
- Timestamp: 12:21:09:022_2
- RFN: 2668
- Chip: 16640
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB5_LongNeighCellInfo LINE 52
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . LastSegmentShort
. . . . . . (SIB_Type)sib_Type[0] = 5
. . . . . . (IntegerType)segmentIndex[-1] = 2
. . . . . . (BitStringType)sib_Data_variable[-1] = "010001011100101011010110100000000000011110001000011000000001011011011011011000100000000001000011000010001001010000001011011010000000010000"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 1c 02 01 03 02 01 ff 00 06 51 89 45 ca d6 80 07 88 60 16 db 62 00 43 08 94 0b 68 04 00

- No.: 1576
- Timestamp: 12:21:09:026_0
- RFN: 2668
- Chip: 31488
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 2
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 03 02 01 ff 0a 01 00 30 06 02 01 06 02 01 02

- No.: 1581
- Timestamp: 12:21:09:032_0
- RFN: 2669
- Chip: 14336
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB6_LongNeighCellInfo LINE 8
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 03 02 01 ff

- No.: 1584
- Timestamp: 12:21:09:033_0
- RFN: 2669
- Chip: 18176
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB6_LongNeighCellInfo:lt_CompleteSIB LINE 4
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 6
. . . . . . . (BitStringType)sib_Data_variable[-1] = "0000001010010001"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 0c 02 01 03 02 01 ff 00 0e 06 0f 02 91

- No.: 1589
- Timestamp: 12:21:09:034_0
- RFN: 2669
- Chip: 22528
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 3
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 03 02 01 ff 0a 01 00 30 06 02 01 06 02 01 03

- No.: 1594
- Timestamp: 12:21:09:041_0
- RFN: 2670
- Chip: 12288
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB6_LongNeighCellInfo LINE 11
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 03 02 01 ff

- No.: 1595
- Timestamp: 12:21:09:042_0
- RFN: 2670
- Chip: 14336
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB6_LongNeighCellInfo LINE 12
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 08 02 01 03 02 01 ff 00 00

- No.: 1599
- Timestamp: 12:21:09:043_0
- RFN: 2670
- Chip: 17664
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 5
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 03 02 01 ff 0a 01 00 30 06 02 01 06 02 01 05

- No.: 1604
- Timestamp: 12:21:09:051_0
- RFN: 2671
- Chip: 12288
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB6_LongNeighCellInfo LINE 14
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 03 02 01 ff

- No.: 1605
- Timestamp: 12:21:09:052_0
- RFN: 2671
- Chip: 14848
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB6_LongNeighCellInfo LINE 15
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 08 02 01 03 02 01 ff 00 00

- No.: 1609
- Timestamp: 12:21:09:053_0
- RFN: 2671
- Chip: 18432
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 6
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 03 02 01 ff 0a 01 00 30 06 02 01 06 02 01 06

- No.: 1614
- Timestamp: 12:21:09:061_0
- RFN: 2672
- Chip: 11520
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB6_LongNeighCellInfo LINE 17
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 03 02 01 ff

- No.: 1615
- Timestamp: 12:21:09:061_1
- RFN: 2672
- Chip: 13312
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB6_LongNeighCellInfo LINE 18
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 08 02 01 03 02 01 ff 00 00

- No.: 1623
- Timestamp: 12:21:09:065_0
- RFN: 2672
- Chip: 25600
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 15
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 03 02 01 ff 0a 01 00 30 06 02 01 06 02 01 0f

- No.: 1628
- Timestamp: 12:21:09:071_0
- RFN: 2673
- Chip: 12800
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB7_LongNeighCellInfo LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 03 02 01 ff

- No.: 1632
- Timestamp: 12:21:09:073_0
- RFN: 2673
- Chip: 17664
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB7_LongNeighCellInfo:lt_CompleteSIB7OrLastSIB12_CompleteSIB7 LINE 9
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 7
. . . . . . . (BitStringType)sib_Data_variable[-1] = "100000101000000010000001"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 0d 02 01 03 02 01 ff 00 0e 07 17 82 80 81

- No.: 1640
- Timestamp: 12:21:09:075_1
- RFN: 2673
- Chip: 28672
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 7
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 03 02 01 ff 0a 01 00 30 06 02 01 06 02 01 07

- No.: 1645
- Timestamp: 12:21:09:081_0
- RFN: 2674
- Chip: 13056
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB7_LongNeighCellInfo:lt_ConcatWithSIB3 LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 03 02 01 ff

- No.: 1646
- Timestamp: 12:21:09:082_0
- RFN: 2674
- Chip: 16640
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB7_LongNeighCellInfo:lt_ConcatWithSIB3 LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 7
. . . . . . . (BitStringType)sib_Data_variable[-1] = "100000101000000010000001"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 3
. . . . . . . (BitStringType)sib_Data_variable[-1] = "010000000000000000000000000011001011001100011000010000000000001000000100011111111111111111111111"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 1b 02 01 03 02 01 ff 00 0e 27 17 82 80 81 1a fa 00 00 00 65 98 c2 00 10 23 ff ff f8

- No.: 1654
- Timestamp: 12:21:09:085_0
- RFN: 2674
- Chip: 26624
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 23
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 03 02 01 ff 0a 01 00 30 06 02 01 06 02 01 17

- No.: 1659
- Timestamp: 12:21:09:091_0
- RFN: 2675
- Chip: 13056
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB7_LongNeighCellInfo:lt_ConcatWithSIB18 LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 03 02 01 ff

- No.: 1660
- Timestamp: 12:21:09:092_0
- RFN: 2675
- Chip: 16128
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB7_LongNeighCellInfo:lt_ConcatWithSIB18 LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 7
. . . . . . . (BitStringType)sib_Data_variable[-1] = "100000101000000010000001"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 26
. . . . . . . (BitStringType)sib_Data_variable[-1] = "100010000111000000000001000000001100000000000100000000110000000000010000000011000000000011000100001"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 1b 02 01 03 02 01 ff 00 0e 27 17 82 80 81 d3 14 43 80 08 06 00 20 18 00 80 60 06 21

- No.: 1668
- Timestamp: 12:21:09:096_2
- RFN: 2675
- Chip: 32256
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 31
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 03 02 01 ff 0a 01 00 30 06 02 01 06 02 01 1f

- No.: 1673
- Timestamp: 12:21:09:101_0
- RFN: 2676
- Chip: 14080
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB7_LongNeighCellInfo:lt_ConcatWithSIB4 LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 03 02 01 ff

- No.: 1674
- Timestamp: 12:21:09:102_0
- RFN: 2676
- Chip: 17152
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB7_LongNeighCellInfo:lt_ConcatWithSIB4 LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 7
. . . . . . . (BitStringType)sib_Data_variable[-1] = "100000101000000010000001"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 4
. . . . . . . (BitStringType)sib_Data_variable[-1] = "0000000000000000000000000001100101100110001100001000000000000100000010001110111"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 19 02 01 03 02 01 ff 00 0e 27 17 82 80 81 22 70 00 00 00 cb 31 84 00 20 47 70

- No.: 1688
- Timestamp: 12:21:09:107_0
- RFN: 2676
- Chip: 31232
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 30
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 03 02 01 ff 0a 01 00 30 06 02 01 06 02 01 1e

- No.: 1693
- Timestamp: 12:21:09:112_0
- RFN: 2677
- Chip: 14080
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB11_LongNeighCellInfo LINE 41
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 03 02 01 ff

- No.: 1694
- Timestamp: 12:21:09:113_0
- RFN: 2677
- Chip: 16384
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB11_LongNeighCellInfo LINE 42
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 08 02 01 03 02 01 ff 00 00

- No.: 1698
- Timestamp: 12:21:09:114_1
- RFN: 2677
- Chip: 19968
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 27
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 03 02 01 ff 0a 01 00 30 06 02 01 06 02 01 1b

- No.: 1703
- Timestamp: 12:21:09:122_0
- RFN: 2678
- Chip: 11264
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB11_LongNeighCellInfo LINE 44
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 03 02 01 ff

- No.: 1704
- Timestamp: 12:21:09:122_1
- RFN: 2678
- Chip: 14080
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB11_LongNeighCellInfo LINE 45
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . SubsequentSegment
. . . . . . (SIB_Type)sib_Type[0] = 11
. . . . . . (IntegerType)segmentIndex[-1] = 1
. . . . . . (BitStringType)sib_Data_fixed[222] = "101000100000101000010000110000100101001001101010100001100001001010100100110000001100101100011011010010100001100101000110010000110110010100011100110100000000010000010010100100101100011011001010001110011010000000001000010001"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 25 02 01 03 02 01 ff 00 04 b0 a2 0a 10 c2 52 6a 86 12 a4 c0 cb 1b 4a 19 46 43 65 1c d0 04 12 92 c6 ca 39 a0 08 44

- No.: 1708
- Timestamp: 12:21:09:124_0
- RFN: 2678
- Chip: 18176
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 26
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 03 02 01 ff 0a 01 00 30 06 02 01 06 02 01 1a

- No.: 1713
- Timestamp: 12:21:09:132_0
- RFN: 2679
- Chip: 13312
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB11_LongNeighCellInfo LINE 47
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 03 02 01 ff

- No.: 1714
- Timestamp: 12:21:09:133_0
- RFN: 2679
- Chip: 16128
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB11_LongNeighCellInfo LINE 48
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . FirstSegment
. . . . . . (SIB_Type)sib_Type[0] = 11
. . . . . . (IntegerType)seg_Count[-1] = 3
. . . . . . (BitStringType)sib_Data_fixed[222] = "001000001101100100001010001100001001100100000100100001010100101100101101100101000111001101000000000100101001010101011110101101100101000111001101000000000000100010001000110010010101010000000100101000010100101010000110000100"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 25 02 01 03 02 01 ff 00 02 b2 20 d9 0a 30 99 04 85 4b 2d 94 73 40 12 95 5e b6 51 cd 00 08 88 c9 54 04 a1 4a 86 10

- No.: 1718
- Timestamp: 12:21:09:134_1
- RFN: 2679
- Chip: 20480
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 29
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 03 02 01 ff 0a 01 00 30 06 02 01 06 02 01 1d

- No.: 1723
- Timestamp: 12:21:09:142_0
- RFN: 2680
- Chip: 11776
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB11_LongNeighCellInfo LINE 50
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 03 02 01 ff

- No.: 1725
- Timestamp: 12:21:09:143_0
- RFN: 2680
- Chip: 15616
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB11_LongNeighCellInfo LINE 52
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . LastSegmentShort
. . . . . . (SIB_Type)sib_Type[0] = 11
. . . . . . (IntegerType)segmentIndex[-1] = 2
. . . . . . (BitStringType)sib_Data_variable[-1] = "01001100100000110110010100011100110100000000011001100110010111110001101001101001110010100100101100011011001010001110011010000000001000111001010111000010001101100101000111001101000000000"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 22 02 01 03 02 01 ff 00 06 b1 b8 4c 83 65 1c d0 06 66 5f 1a 69 ca 4b 1b 28 e6 80 23 95 c2 36 51 cd 00 00

- No.: 1738
- Timestamp: 12:21:09:146_3
- RFN: 2680
- Chip: 29184
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 13
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 03 02 01 ff 0a 01 00 30 06 02 01 06 02 01 0d

- No.: 1743
- Timestamp: 12:21:09:152_0
- RFN: 2681
- Chip: 12544
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB12_LongNeighCellInfo LINE 41
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 03 02 01 ff

- No.: 1744
- Timestamp: 12:21:09:153_0
- RFN: 2681
- Chip: 15616
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB12_LongNeighCellInfo LINE 42
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . SubsequentSegment
. . . . . . (SIB_Type)sib_Type[0] = 12
. . . . . . (IntegerType)segmentIndex[-1] = 1
. . . . . . (BitStringType)sib_Data_fixed[222] = "110000100101001001101010100001100001001010100100110000001100101100011011010010100001100101000110010010110110010100011100110100000000010000010010100100101101011011001010001110011010000000001000010001010011001000101101100101"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 25 02 01 03 02 01 ff 00 04 c0 c2 52 6a 86 12 a4 c0 cb 1b 4a 19 46 4b 65 1c d0 04 12 92 d6 ca 39 a0 08 45 32 2d 94

- No.: 1748
- Timestamp: 12:21:09:154_0
- RFN: 2681
- Chip: 19456
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 11
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 03 02 01 ff 0a 01 00 30 06 02 01 06 02 01 0b

- No.: 1753
- Timestamp: 12:21:09:162_0
- RFN: 2682
- Chip: 11776
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB12_LongNeighCellInfo LINE 44
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 03 02 01 ff

- No.: 1754
- Timestamp: 12:21:09:162_1
- RFN: 2682
- Chip: 14848
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB12_LongNeighCellInfo LINE 45
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . FirstSegment
. . . . . . (SIB_Type)sib_Type[0] = 12
. . . . . . (IntegerType)seg_Count[-1] = 3
. . . . . . (BitStringType)sib_Data_fixed[222] = "000000011011001000001100100001010100101100101101100101000111001101000000000100101001010101011110101101100101000111001101000000000000100010001000110010010101010000000100101000010100100000000110000100101000100000101000010000"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 25 02 01 03 02 01 ff 00 02 c2 01 b2 0c 85 4b 2d 94 73 40 12 95 5e b6 51 cd 00 08 88 c9 54 04 a1 48 06 12 88 28 40

- No.: 1758
- Timestamp: 12:21:09:164_0
- RFN: 2682
- Chip: 18688
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 15
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 03 02 01 ff 0a 01 00 30 06 02 01 06 02 01 0f

- No.: 1763
- Timestamp: 12:21:09:172_0
- RFN: 2683
- Chip: 13056
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB12_LongNeighCellInfo LINE 47
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 03 02 01 ff

- No.: 1768
- Timestamp: 12:21:09:174_0
- RFN: 2683
- Chip: 21248
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB12_LongNeighCellInfo:lt_CompleteSIB7 LINE 7
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 7
. . . . . . . (BitStringType)sib_Data_variable[-1] = "100000101000000010000001"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 0d 02 01 03 02 01 ff 00 0e 07 17 82 80 81

- No.: 1773
- Timestamp: 12:21:09:175_3
- RFN: 2683
- Chip: 25600
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 14
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 03 02 01 ff 0a 01 00 30 06 02 01 06 02 01 0e

- No.: 1778
- Timestamp: 12:21:09:182_0
- RFN: 2684
- Chip: 11776
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB12_LongNeighCellInfo LINE 50
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 03 02 01 ff

- No.: 1780
- Timestamp: 12:21:09:182_2
- RFN: 2684
- Chip: 14848
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB12_LongNeighCellInfo LINE 52
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . LastSegmentShort
. . . . . . (SIB_Type)sib_Type[0] = 12
. . . . . . (IntegerType)segmentIndex[-1] = 2
. . . . . . (BitStringType)sib_Data_variable[-1] = "00011100110100000000011001100110010111110001101001101001110010100100101101011011001010001110011010000000001000111001010111000010101101100101000111001101000000000"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 1f 02 01 03 02 01 ff 00 06 c1 a0 1c d0 06 66 5f 1a 69 ca 4b 5b 28 e6 80 23 95 c2 b6 51 cd 00 00

- No.: 1788
- Timestamp: 12:21:09:185_4
- RFN: 2684
- Chip: 25856
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 23
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 03 02 01 ff 0a 01 00 30 06 02 01 06 02 01 17

- No.: 1793
- Timestamp: 12:21:09:192_0
- RFN: 2685
- Chip: 12800
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB18_LongNeighCellInfo LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 03 02 01 ff

- No.: 1794
- Timestamp: 12:21:09:193_0
- RFN: 2685
- Chip: 15616
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB18_LongNeighCellInfo LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 7
. . . . . . . (BitStringType)sib_Data_variable[-1] = "100000101000000010000001"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 26
. . . . . . . (BitStringType)sib_Data_variable[-1] = "100010000111000000000001000000001100000000000100000000110000000000010000000011000000000011000100001"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 1b 02 01 03 02 01 ff 00 0e 27 17 82 80 81 d3 14 43 80 08 06 00 20 18 00 80 60 06 21

- No.: 1806
- Timestamp: 12:21:09:195_3
- RFN: 2685
- Chip: 26112
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 4
. . (IntegerType)sg_POS[-1] = 1
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 03 02 01 ff 0a 01 00 30 06 02 01 04 02 01 01

- No.: 1811
- Timestamp: 12:21:09:202_0
- RFN: 2686
- Chip: 11776
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSB1_LongNeighCellInfo LINE 4
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 03 02 01 ff

- No.: 1814
- Timestamp: 12:21:09:203_0
- RFN: 2686
- Chip: 15872
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSB1_LongNeighCellInfo:lt_CompleteSIB LINE 4
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 27
. . . . . . . (BitStringType)sib_Data_variable[-1] = "0001000010101000100000100011000001011101010011100100100110100001000000010101101110010010001011000100010000110010100010010111"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 1a 02 01 03 02 01 ff 00 0e 1b 7b 10 a8 82 30 5d 4e 49 a1 01 5b 92 2c 44 32 89 70

- No.: 1832
- Timestamp: 12:21:09:206_3
- RFN: 2686
- Chip: 29952
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 3
. . (IntegerType)sg_POS[-1] = 0
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 03 02 01 ff 0a 01 00 30 06 02 01 03 02 01 00

- No.: 1837
- Timestamp: 12:21:09:212_0
- RFN: 2687
- Chip: 12800
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendMIB LINE 7
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 03 02 01 ff

- No.: 1840
- Timestamp: 12:21:09:213_0
- RFN: 2687
- Chip: 16384
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendMIB:lt_CompleteSIB LINE 4
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 0
. . . . . . . (BitStringType)sib_Data_variable[-1] = "0001000000000000100000100010010110101010000100010000000000001000100010100000101000100010100001001000100001110001101000100111110010001110010010010010000100000001"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 1e 02 01 03 02 01 ff 00 0e 00 9f 10 00 82 25 aa 11 00 08 8a 0a 22 84 88 71 a2 7c 8e 49 21 01

- No.: 1847
- Timestamp: 12:21:09:214_2
- RFN: 2687
- Chip: 20480
- Event: Start Timer
- Source: ts_RRC_Delay LINE 1
- Message Structure:
no details available
- Constraint:
t_Dly (5000 Ms)
- BinaryMessage:

- No.: 1851
- Timestamp: 12:21:14:207_0
- RFN: 3186
- Chip: 35072
- Event: Timeout
- Source: ts_RRC_Delay LINE 2
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 1863
- Timestamp: 12:21:14:210_0
- RFN: 3187
- Chip: 5632
- Event: Send
- PCO: CMAC
- Message: CMAC_PAGING_Config_REQ
- Source: ts_CMAC_Pag1_Cfg LINE 4
- Message Structure:
CMAC_PAGING_Config_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 5
. (RatType)ratType[0] = 0
. CmacPagingConfigReq
. . pI_BitMapInfo
. . . (BitStringType)e18[18] = '010000000000000000'B
. . (IntegerType)dRX_CycleLength[-1] = 7
. . IMSI_GSM_MAP
. . . (IntegerType)_elem[-1] = 0
. . . (IntegerType)_elem[-1] = 0
. . . (IntegerType)_elem[-1] = 1
. . . (IntegerType)_elem[-1] = 0
. . . (IntegerType)_elem[-1] = 1
. . . (IntegerType)_elem[-1] = 0
. . . (IntegerType)_elem[-1] = 1
. . . (IntegerType)_elem[-1] = 2
. . . (IntegerType)_elem[-1] = 3
. . . (IntegerType)_elem[-1] = 4
. . . (IntegerType)_elem[-1] = 5
. . . (IntegerType)_elem[-1] = 6
. . . (IntegerType)_elem[-1] = 0
. . . (IntegerType)_elem[-1] = 6
. . . (IntegerType)_elem[-1] = 3
. . (BooleanType)t_pich_T_sccpch = FALSE
- Constraint:
ca_CMAC_PagingCfgReq
- BinaryMessage:
30 46 02 01 03 02 01 05 0a 01 00 30 3b 03 04 06 40 40 40 02 01 07 30 2d 02 01 00 02 01 00 02 01 01 02 01 00 02 01 01 02 01 00 02 01 01 02 01 02 02 01 03 02 01 04 02 01 05 02 01 06 02 01 00 02 01 06 02 01 03 01 01 00

- No.: 1867
- Timestamp: 12:21:14:212_0
- RFN: 3187
- Chip: 14336
- Event: Receive
- PCO: CMAC
- Message: CMAC_PAGING_Config_CNF
- Source: ts_CMAC_Pag1_Cfg LINE 5
- Message Structure:
CMAC_PAGING_Config_CNF
. (IntegerType)cellId[0] = 3
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 5
- Constraint:
ca_CMAC_PagingCfgCnf
- BinaryMessage:
30 06 02 01 03 02 01 05

- No.: 1869
- Timestamp: 12:21:14:213_0
- RFN: 3187
- Chip: 17408
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendPage1_ModifySI LINE 3
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -2
. tM_message
. . PCCH_Message
. . . PCCH_MessageType
. . . . PagingType1
. . . . . PagingRecordList
. . . . . BCCH_ModificationInfo
. . . . . . (IntegerType)mib_ValueTag[-1] = 2
. . . . . . (IntegerType)bcch_ModificationTime[-1] = -
. . . . . laterNonCriticalExtensions
- Constraint:
cas_PagingType1
- BinaryMessage:
30 07 02 01 03 02 01 fe 21

- No.: 1923
- Timestamp: 12:21:14:220_0
- RFN: 3188
- Chip: 6400
- Event: Send
- PCO: CPHY
- Message: CPHY_Cell_Config_REQ
- Source: ts_SS_CellCfg LINE 6
- Message Structure:
CPHY_Cell_Config_REQ
. (IntegerType)cellId[-1] = 6
. (IntegerType)tcell[-1] = 7253
. (IntegerType)sfnOffset[-1] = 0
. FrequencyInfo
. . modeSpecificInfo
. . . FrequencyInfoFDD
. . . . (IntegerType)uarfcn_UL[-1] = 9713
. . . . (IntegerType)uarfcn_DL[-1] = 10663
. (IntegerType)primaryScramblingCode_SS[-1] = 150
. CellTxPowerLevel
. (IntegerType)dLTxAttenuationLevel[-1] = 8
- Constraint:
ca_CellCfgReq
- BinaryMessage:
30 1f 02 01 06 02 02 1c 55 02 01 00 30 0a 30 08 02 02 25 f1 02 02 29 a7 02 02 00 96 05 00 02 01 08

- No.: 1927
- Timestamp: 12:21:14:616_0
- RFN: 3227
- Chip: 30976
- Event: Receive
- PCO: CPHY
- Message: CPHY_Cell_Config_CNF
- Source: ts_SS_CellCfg LINE 7
- Message Structure:
CPHY_Cell_Config_CNF
. (IntegerType)cellId[0] = 6
- Constraint:
ca_CellCfgCnf
- BinaryMessage:
30 03 02 01 06

- No.: 1939
- Timestamp: 12:21:14:618_0
- RFN: 3228
- Chip: 512
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 3
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 0
. (RatType)ratType[0] = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . PrimaryCPICHInfo
. . . . (IntegerType)dl_TxPower_PCPICH[-1] = -60
. . . . (BooleanType)txdiversityIndicator = FALSE
- Constraint:
ca_pCPICH_Info
- BinaryMessage:
30 13 02 01 06 02 01 00 0a 01 00 30 08 30 06 02 01 c4 01 01 00

- No.: 1943
- Timestamp: 12:21:14:627_0
- RFN: 3228
- Chip: 34048
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 4
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId[0] = 6
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 0
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 06 02 01 00

- No.: 1944
- Timestamp: 12:21:14:627_1
- RFN: 3228
- Chip: 36608
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 5
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 1
. (RatType)ratType[0] = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . PrimarySCHInfo
. . . . (BooleanType)tstdIndicator = FALSE
. . . . (IntegerType)dl_TxPower[-1] = -5
- Constraint:
ca_pSCH_Info
- BinaryMessage:
30 13 02 01 06 02 01 01 0a 01 00 30 08 30 06 01 01 00 02 01 fb

- No.: 1948
- Timestamp: 12:21:14:634_0
- RFN: 3229
- Chip: 25344
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 6
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId[0] = 6
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 1
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 06 02 01 01

- No.: 1949
- Timestamp: 12:21:14:635_0
- RFN: 3229
- Chip: 27904
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 7
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 2
. (RatType)ratType[0] = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . SecondarySCHInfo
. . . . (BooleanType)tstdIndicator = FALSE
. . . . (IntegerType)dl_TxPower[-1] = -5
- Constraint:
ca_sSCH_Info
- BinaryMessage:
30 13 02 01 06 02 01 02 0a 01 00 30 08 30 06 01 01 00 02 01 fb

- No.: 1953
- Timestamp: 12:21:14:775_0
- RFN: 3243
- Chip: 24576
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 8
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId[0] = 6
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 2
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 06 02 01 02

- No.: 1954
- Timestamp: 12:21:14:775_1
- RFN: 3243
- Chip: 27648
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 9
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 4
. (RatType)ratType[0] = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . PrimaryCCPCHInfo
. . . . (BooleanType)sttd_Indicator = FALSE
. . . . (IntegerType)dl_TxPower[-1] = -2
- Constraint:
ca_pCCPCH_Info
- BinaryMessage:
30 13 02 01 06 02 01 04 0a 01 00 30 08 30 06 01 01 00 02 01 fe

- No.: 1958
- Timestamp: 12:21:14:783_0
- RFN: 3244
- Chip: 17664
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 10
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId[0] = 6
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 4
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 06 02 01 04

- No.: 1959
- Timestamp: 12:21:14:785_0
- RFN: 3244
- Chip: 25856
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Config_REQ
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 11
- Message Structure:
CPHY_TrCH_Config_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 4
. (RatType)ratType[0] = 0
. TrChConfigType
. CphyTrchConfigReq
. . SS_ActivationTime
. . ulconnectedTrCHList
. . TFCS
. . dlconnectedTrCHList
. . . CphyTrchConfigReq_setseq_1
. . . . (IntegerType)trchid[-1] = 11
. . . . (SS_DL_TransportChannelType)dl_TransportChannelType[0] = 2
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size[-1] = 246
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional[0] = 0
. . . . . . (IntegerType)rateMatchingAttribute[-1] = 1
. . . . . . (CRC_Size)crc_Size[0] = 3
. . TFCS
. . . ExplicitTFCS_Configuration
. . . . TFCS_ReconfAdd
. . . . . ctfcSize
. . . . . . ctfc2Bit
. . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . (IntegerType)ctfc2[-1] = 0
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . fdd
. . . . . . . . . . . . . (IntegerType)gainFactorBetaC[-1] = 11
. . . . . . . . . . . (IntegerType)gainFactorBetaD[-1] = 15
. . . . . . . . . . . (IntegerType)referenceTFC_ID[-1] = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
- Constraint:
ca_BCH_InfoActNow
- BinaryMessage:
30 4c 02 01 06 02 01 04 0a 01 00 05 00 30 3f 05 00 30 23 30 21 02 01 0b 0a 01 02 30 19 30 0c 30 0a 02 02 00 f6 30 02 05 00 05 00 30 09 0a 01 00 02 01 01 0a 01 03 30 16 30 14 30 12 02 01 00 30 0d 30 0b 30 03 02 01 0b 02 01 0f 02 01 00

- No.: 1963
- Timestamp: 12:21:14:794_0
- RFN: 3245
- Chip: 22272
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Config_CNF
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 12
- Message Structure:
CPHY_TrCH_Config_CNF
. (IntegerType)cellId[0] = 6
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 4
- Constraint:
ca_TrChCfgCnf
- BinaryMessage:
30 06 02 01 06 02 01 04

- No.: 1964
- Timestamp: 12:21:14:798_0
- RFN: 3245
- Chip: 37632
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 13
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 4
. (RatType)ratType[0] = 0
. configMessage
. . CmacConfigReq
. . . SS_ActivationTime
. . . UE_Info
. . . . U_RNTI
. . . . (BitStringType)c_RNTI[16] = -
. . . TrCHInfo
. . . . ulconnectedTrCHList
. . . . TFCS
. . . . dlconnectedTrCHList
. . . . . TrCHInfo_setseq_1
. . . . . . (IntegerType)trchid[-1] = 11
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size[-1] = 246
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional[0] = 0
. . . . . . . . (IntegerType)rateMatchingAttribute[-1] = 1
. . . . . . . . (CRC_Size)crc_Size[0] = 3
. . . . TFCS
. . . . . ExplicitTFCS_Configuration
. . . . . . TFCS_ReconfAdd
. . . . . . . ctfcSize
. . . . . . . . ctfc2Bit
. . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . (IntegerType)ctfc2[-1] = 0
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC[-1] = 11
. . . . . . . . . . . . . (IntegerType)gainFactorBetaD[-1] = 15
. . . . . . . . . . . . . (IntegerType)referenceTFC_ID[-1] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . TrCH_LogCHMappingList1
. . . . ulconnectedTrCHList
. . . . dlconnectedTrCHList
. . . . . TrCH_LogCHMappingList1_setseq_1
. . . . . . (IntegerType)trchid[-1] = 11
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation[0] = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType[0] = 2
. . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . . . (LogicalChannelType)logicalChannelType[0] = 0
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 1
. . . . . . . . (IntegerType)rB_Identity[-1] = -1
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_CMAC_CfgInfo
- BinaryMessage:
30 6e 02 01 06 02 01 04 0a 01 00 30 63 05 00 30 00 30 3a 30 20 30 1e 02 01 0b 30 19 30 0c 30 0a 02 02 00 f6 30 02 05 00 05 00 30 09 0a 01 00 02 01 01 0a 01 03 30 16 30 14 30 12 02 01 00 30 0d 30 0b 30 03 02 01 0b 02 01 0f 02 01 00 30 21 30 1f 30 1d 02 01 0b 30 18 30 16 30 11 0a 01 00 0a 01 02 02 01 01 0a 01 00 05 00 02 01 01 02 01 ff

- No.: 1968
- Timestamp: 12:21:14:804_0
- RFN: 3246
- Chip: 23552
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_SS_BCH_SCH_CPICH_Cfg LINE 14
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId[0] = 6
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 4
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 06 02 01 04

- No.: 2006
- Timestamp: 12:21:14:809_1
- RFN: 3247
- Chip: 4608
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_PCH_FACH_CCCH_Cfg LINE 3
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 5
. (RatType)ratType[0] = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . SecondaryCCPCHInfo
. . . . (IntegerType)scramblingCode[-1] = 0
. . . . SF256_AndCodeNumber
. . . . . (IntegerType)sf64[-1] = 1
. . . . (IntegerType)sCCPCHSlotFormat[-1] = 8
. . . . (IntegerType)timingOffset[-1] = 0
. . . . (PositionFixedOrFlexible)positionFixedOrFlexible[0] = 1
. . . . (BooleanType)sttd_Indicator = FALSE
. . . . (IntegerType)dl_TxPower[-1] = -2
. . . . (IntegerType)powerOffsetOfTFCI_PO1[-1] = 6
. . . . (IntegerType)powerOffsetOfPILOT_PO3[-1] = 6
- Constraint:
ca_sCCPCH_Info
- BinaryMessage:
30 28 02 01 06 02 01 05 0a 01 00 30 1d 30 1b 02 01 00 02 01 01 02 01 08 02 01 00 0a 01 01 01 01 00 02 01 fe 02 01 06 02 01 06

- No.: 2010
- Timestamp: 12:21:14:816_0
- RFN: 3247
- Chip: 31744
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_PCH_FACH_CCCH_Cfg LINE 4
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId[0] = 6
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 5
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 06 02 01 05

- No.: 2011
- Timestamp: 12:21:14:825_0
- RFN: 3248
- Chip: 27904
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Config_REQ
- Source: ts_SS_PCH_FACH_CCCH_Cfg LINE 5
- Message Structure:
CPHY_TrCH_Config_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 5
. (RatType)ratType[0] = 0
. TrChConfigType
. CphyTrchConfigReq
. . SS_ActivationTime
. . ulconnectedTrCHList
. . TFCS
. . dlconnectedTrCHList
. . . CphyTrchConfigReq_setseq_1
. . . . (IntegerType)trchid[-1] = 12
. . . . (SS_DL_TransportChannelType)dl_TransportChannelType[0] = 3
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size[-1] = 240
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional[0] = 0
. . . . . . (IntegerType)rateMatchingAttribute[-1] = 230
. . . . . . (CRC_Size)crc_Size[0] = 3
. . . CphyTrchConfigReq_setseq_1
. . . . (IntegerType)trchid[-1] = 13
. . . . (SS_DL_TransportChannelType)dl_TransportChannelType[0] = 1
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size[-1] = 168
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . (IntegerType)small[-1] = 2
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional[0] = 0
. . . . . . (IntegerType)rateMatchingAttribute[-1] = 220
. . . . . . (CRC_Size)crc_Size[0] = 3
. . . CphyTrchConfigReq_setseq_1
. . . . (IntegerType)trchid[-1] = 14
. . . . (SS_DL_TransportChannelType)dl_TransportChannelType[0] = 1
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size[-1] = 360
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . (IntegerType)rateMatchingAttribute[-1] = 130
. . . . . . (CRC_Size)crc_Size[0] = 3
. . TFCS
. . . ExplicitTFCS_Configuration
. . . . TFCS_ReconfAdd
. . . . . ctfcSize
. . . . . . ctfc4Bit
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4[-1] = 0
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4[-1] = 1
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4[-1] = 2
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4[-1] = 3
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4[-1] = 4
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4[-1] = 5
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4[-1] = 6
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . (IntegerType)ctfc4[-1] = 8
. . . . . . . . PowerOffsetInformation
. . . . . . . . . GainFactorInformation
. . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . fdd
. . . . . . . . . . . . . (IntegerType)gainFactorBetaC[-1] = 11
. . . . . . . . . . . (IntegerType)gainFactorBetaD[-1] = 15
. . . . . . . . . . . (IntegerType)referenceTFC_ID[-1] = 0
. . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
- Constraint:
ca_PCH_2_FACH_InfoActNow
- BinaryMessage:
30 81 e4 02 01 06 02 01 05 0a 01 00 05 00 30 81 d6 05 00 30 74 30 24 02 01 0c 0a 01 03 30 1c 30 0e 30 0c 02 02 00 f0 30 04 05 00 05 00 05 00 30 0a 0a 01 00 02 02 00 e6 0a 01 03 30 27 02 01 0d 0a 01 01 30 1f 30 11 30 0f 02 02 00 a8 30 07 05 00 05 00 02 01 02 05 00 30 0a 0a 01 00 02 02 00 dc 0a 01 03 30 23 02 01 0e 0a 01 01 30 1b 30 0e 30 0c 02 02 01 68 30 04 05 00 05 00 05 00 30 09 05 00 02 02 00 82 0a 01 03 30 5c 30 5a 30 08 02 01 00 30 03 02 01 00 30 08 02 01 01 30 03 02 01 00 30 08 02 01 02 30 03 02 01 00 30 08 02 01 03 30 03 02 01 00 30 08 02 01 04 30 03 02 01 00 30 08 02 01 05 30 03 02 01 00 30 08 02 01 06 30 03 02 01 00 30 12 02 01 08 30 0d 30 0b 30 03 02 01 0b 02 01 0f 02 01 00

- No.: 2015
- Timestamp: 12:21:14:838_0
- RFN: 3249
- Chip: 37120
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Config_CNF
- Source: ts_SS_PCH_FACH_CCCH_Cfg LINE 6
- Message Structure:
CPHY_TrCH_Config_CNF
. (IntegerType)cellId[0] = 6
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 5
- Constraint:
ca_TrChCfgCnf
- BinaryMessage:
30 06 02 01 06 02 01 05

- No.: 2016
- Timestamp: 12:21:14:849_0
- RFN: 3251
- Chip: 3584
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_SS_PCH_FACH_CCCH_Cfg LINE 7
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 5
. (RatType)ratType[0] = 0
. configMessage
. . CmacConfigReq
. . . SS_ActivationTime
. . . UE_Info
. . . . U_RNTI
. . . . (BitStringType)c_RNTI[16] = -
. . . TrCHInfo
. . . . ulconnectedTrCHList
. . . . TFCS
. . . . dlconnectedTrCHList
. . . . . TrCHInfo_setseq_1
. . . . . . (IntegerType)trchid[-1] = 12
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size[-1] = 240
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional[0] = 0
. . . . . . . . (IntegerType)rateMatchingAttribute[-1] = 230
. . . . . . . . (CRC_Size)crc_Size[0] = 3
. . . . . TrCHInfo_setseq_1
. . . . . . (IntegerType)trchid[-1] = 13
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size[-1] = 168
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . (IntegerType)small[-1] = 2
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional[0] = 0
. . . . . . . . (IntegerType)rateMatchingAttribute[-1] = 220
. . . . . . . . (CRC_Size)crc_Size[0] = 3
. . . . . TrCHInfo_setseq_1
. . . . . . (IntegerType)trchid[-1] = 14
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size[-1] = 360
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . (IntegerType)rateMatchingAttribute[-1] = 130
. . . . . . . . (CRC_Size)crc_Size[0] = 3
. . . . TFCS
. . . . . ExplicitTFCS_Configuration
. . . . . . TFCS_ReconfAdd
. . . . . . . ctfcSize
. . . . . . . . ctfc4Bit
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4[-1] = 0
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4[-1] = 1
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4[-1] = 2
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4[-1] = 3
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4[-1] = 4
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4[-1] = 5
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4[-1] = 6
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4[-1] = 8
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC[-1] = 11
. . . . . . . . . . . . . (IntegerType)gainFactorBetaD[-1] = 15
. . . . . . . . . . . . . (IntegerType)referenceTFC_ID[-1] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . TrCH_LogCHMappingList1
. . . . ulconnectedTrCHList
. . . . dlconnectedTrCHList
. . . . . TrCH_LogCHMappingList1_setseq_1
. . . . . . (IntegerType)trchid[-1] = 12
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation[0] = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType[0] = 3
. . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . . . (LogicalChannelType)logicalChannelType[0] = 1
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 1
. . . . . . . . (IntegerType)rB_Identity[-1] = -2
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
. . . . . TrCH_LogCHMappingList1_setseq_1
. . . . . . (IntegerType)trchid[-1] = 13
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation[0] = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType[0] = 1
. . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 5
. . . . . . . . . . (LogicalChannelType)logicalChannelType[0] = 2
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 1
. . . . . . . . (IntegerType)rB_Identity[-1] = 0
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_CMAC_CfgInfo
- BinaryMessage:
30 82 01 21 02 01 06 02 01 05 0a 01 00 30 82 01 14 05 00 30 00 30 81 cb 30 6b 30 21 02 01 0c 30 1c 30 0e 30 0c 02 02 00 f0 30 04 05 00 05 00 05 00 30 0a 0a 01 00 02 02 00 e6 0a 01 03 30 24 02 01 0d 30 1f 30 11 30 0f 02 02 00 a8 30 07 05 00 05 00 02 01 02 05 00 30 0a 0a 01 00 02 02 00 dc 0a 01 03 30 20 02 01 0e 30 1b 30 0e 30 0c 02 02 01 68 30 04 05 00 05 00 05 00 30 09 05 00 02 02 00 82 0a 01 03 30 5c 30 5a 30 08 02 01 00 30 03 02 01 00 30 08 02 01 01 30 03 02 01 00 30 08 02 01 02 30 03 02 01 00 30 08 02 01 03 30 03 02 01 00 30 08 02 01 04 30 03 02 01 00 30 08 02 01 05 30 03 02 01 00 30 08 02 01 06 30 03 02 01 00 30 12 02 01 08 30 0d 30 0b 30 03 02 01 0b 02 01 0f 02 01 00 30 40 30 3e 30 1d 02 01 0c 30 18 30 16 30 11 0a 01 00 0a 01 03 02 01 01 0a 01 01 05 00 02 01 01 02 01 fe 30 1d 02 01 0d 30 18 30 16 30 11 0a 01 00 0a 01 01 02 01 05 0a 01 02 05 00 02 01 01 02 01 00

- No.: 2020
- Timestamp: 12:21:14:858_0
- RFN: 3252
- Chip: 1024
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_SS_PCH_FACH_CCCH_Cfg LINE 8
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId[0] = 6
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 5
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 06 02 01 05

- No.: 2021
- Timestamp: 12:21:14:859_0
- RFN: 3252
- Chip: 5888
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_PCH_FACH_CCCH_Cfg LINE 9
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 6
. (RatType)ratType[0] = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . PICHInfo
. . . . PICH_Info
. . . . . fdd
. . . . . . (IntegerType)channelisationCode256[-1] = 2
. . . . . . (PI_CountPerFrame)pi_CountPerFrame[0] = 0
. . . . . . (BooleanType)sttd_Indicator = FALSE
. . . . (IntegerType)dl_TxPower[-1] = -5
. . . . (IntegerType)sccpchId_associated[-1] = 5
- Constraint:
ca_PICH_Info
- BinaryMessage:
30 1e 02 01 06 02 01 06 0a 01 00 30 13 30 11 30 09 02 01 02 0a 01 00 01 01 00 02 01 fb 02 01 05

- No.: 2025
- Timestamp: 12:21:14:869_0
- RFN: 3253
- Chip: 3840
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_PCH_FACH_CCCH_Cfg LINE 10
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId[0] = 6
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 6
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 06 02 01 06

- No.: 2033
- Timestamp: 12:21:14:871_0
- RFN: 3253
- Chip: 12288
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_RACH_CCCH_Cfg LINE 3
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 7
. (RatType)ratType[0] = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . AICHInfo
. . . . AICH_Info
. . . . . (IntegerType)channelisationCode256[-1] = 3
. . . . . (BooleanType)sttd_Indicator = FALSE
. . . . . (AICH_TransmissionTiming)aich_TransmissionTiming[0] = 0
. . . . (IntegerType)dl_TxPower[-1] = -5
- Constraint:
ca_AichInfo
- BinaryMessage:
30 1b 02 01 06 02 01 07 0a 01 00 30 10 30 0e 30 09 02 01 03 01 01 00 0a 01 00 02 01 fb

- No.: 2037
- Timestamp: 12:21:14:884_0
- RFN: 3254
- Chip: 24064
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_RACH_CCCH_Cfg LINE 4
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId[0] = 6
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 7
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 06 02 01 07

- No.: 2038
- Timestamp: 12:21:14:886_0
- RFN: 3254
- Chip: 29696
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Setup_REQ
- Source: ts_SS_RACH_CCCH_Cfg LINE 5
- Message Structure:
CPHY_RL_Setup_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 8
. (RatType)ratType[0] = 0
. CphyRlSetupReq
. . physicalChannelInfo
. . . PRACHInfo
. . . . fdd_tdd
. . . . . fdd
. . . . . . (BitStringType)preambleSignature[16] = "0000000011111111"
. . . . . . (SF_PRACH)spreadingFactorForDataPart[0] = 1
. . . . . . (IntegerType)preambleScramblingCode[-1] = 0
. . . . . . (PuncturingLimit)puncturingLimit[0] = 15
. . . . . . (BitStringType)accessSlot[12] = "111111111111"
- Constraint:
ca_PRACH_Info
- BinaryMessage:
30 22 02 01 06 02 01 08 0a 01 00 30 17 30 15 30 13 03 03 00 00 00 0a 01 01 02 01 00 0a 01 0f 03 03 04 ff ff

- No.: 2042
- Timestamp: 12:21:14:895_0
- RFN: 3255
- Chip: 28160
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Setup_CNF
- Source: ts_SS_RACH_CCCH_Cfg LINE 6
- Message Structure:
CPHY_RL_Setup_CNF
. (IntegerType)cellId[0] = 6
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 8
- Constraint:
ca_RL_SetupCnf
- BinaryMessage:
30 06 02 01 06 02 01 08

- No.: 2043
- Timestamp: 12:21:14:899_0
- RFN: 3256
- Chip: 3072
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Config_REQ
- Source: ts_SS_RACH_CCCH_Cfg LINE 7
- Message Structure:
CPHY_TrCH_Config_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 8
. (RatType)ratType[0] = 0
. TrChConfigType
. CphyTrchConfigReq
. . SS_ActivationTime
. . ulconnectedTrCHList
. . . CphyTrchConfigReq_setseq_0
. . . . (IntegerType)trchid[-1] = 15
. . . . (SS_UL_TransportChannelType)ul_TransportChannelType[0] = 1
. . . . CommonOrDedicatedTFS
. . . . . tti
. . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size[-1] = 168
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . (IntegerType)tb_Size[-1] = 360
. . . . . . . . numberOfTbSizeList
. . . . . . . . . NumberOfTransportBlocks
. . . . . . . . LogicalChannelList
. . . . . SemistaticTF_Information
. . . . . . ChannelCodingType
. . . . . . . (CodingRate)convolutional[0] = 0
. . . . . . (IntegerType)rateMatchingAttribute[-1] = 150
. . . . . . (CRC_Size)crc_Size[0] = 3
. . TFCS
. . . ExplicitTFCS_Configuration
. . . . TFCS_ReconfAdd
. . . . . ctfcSize
. . . . . . ctfc2Bit
. . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . (IntegerType)ctfc2[-1] = 0
. . . . . . . . PowerOffsetInformation
. . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . (IntegerType)ctfc2[-1] = 1
. . . . . . . . PowerOffsetInformation
. . dlconnectedTrCHList
. . TFCS
- Constraint:
cab_RACH_InfoActNow
- BinaryMessage:
30 4f 02 01 06 02 01 08 0a 01 00 05 00 30 42 05 00 30 30 30 2e 02 01 0f 0a 01 01 30 26 30 18 30 0a 02 02 00 a8 30 02 05 00 05 00 30 0a 02 02 01 68 30 02 05 00 05 00 30 0a 0a 01 00 02 02 00 96 0a 01 03 30 0c 30 0a 30 03 02 01 00 30 03 02 01 01

- No.: 2047
- Timestamp: 12:21:14:915_0
- RFN: 3257
- Chip: 29440
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Config_CNF
- Source: ts_SS_RACH_CCCH_Cfg LINE 8
- Message Structure:
CPHY_TrCH_Config_CNF
. (IntegerType)cellId[0] = 6
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 8
- Constraint:
ca_TrChCfgCnf
- BinaryMessage:
30 06 02 01 06 02 01 08

- No.: 2048
- Timestamp: 12:21:14:920_0
- RFN: 3258
- Chip: 9984
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_SS_RACH_CCCH_Cfg LINE 9
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 8
. (RatType)ratType[0] = 0
. configMessage
. . CmacConfigReq
. . . SS_ActivationTime
. . . UE_Info
. . . . U_RNTI
. . . . (BitStringType)c_RNTI[16] = -
. . . TrCHInfo
. . . . ulconnectedTrCHList
. . . . . TrCHInfo_setseq_0
. . . . . . (IntegerType)trchid[-1] = 15
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size[-1] = 168
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size[-1] = 360
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional[0] = 0
. . . . . . . . (IntegerType)rateMatchingAttribute[-1] = 150
. . . . . . . . (CRC_Size)crc_Size[0] = 3
. . . . TFCS
. . . . . ExplicitTFCS_Configuration
. . . . . . TFCS_ReconfAdd
. . . . . . . ctfcSize
. . . . . . . . ctfc2Bit
. . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . (IntegerType)ctfc2[-1] = 0
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . (IntegerType)ctfc2[-1] = 1
. . . . . . . . . . PowerOffsetInformation
. . . . dlconnectedTrCHList
. . . . TFCS
. . . TrCH_LogCHMappingList1
. . . . ulconnectedTrCHList
. . . . . TrCH_LogCHMappingList1_setseq_0
. . . . . . (IntegerType)trchid[-1] = 15
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation[0] = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType[0] = 1
. . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 5
. . . . . . . . . . (LogicalChannelType)logicalChannelType[0] = 2
. . . . . . . . (IntegerType)rB_Identity[-1] = 0
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
. . . . dlconnectedTrCHList
- Constraint:
ca_CMAC_CfgInfo
- BinaryMessage:
30 6c 02 01 06 02 01 08 0a 01 00 30 61 05 00 30 00 30 3d 30 2d 30 2b 02 01 0f 30 26 30 18 30 0a 02 02 00 a8 30 02 05 00 05 00 30 0a 02 02 01 68 30 02 05 00 05 00 30 0a 0a 01 00 02 02 00 96 0a 01 03 30 0c 30 0a 30 03 02 01 00 30 03 02 01 01 30 1c 30 1a 30 18 02 01 0f 30 13 30 11 30 0c 0a 01 00 0a 01 01 02 01 05 0a 01 02 02 01 00

- No.: 2052
- Timestamp: 12:21:14:925_0
- RFN: 3258
- Chip: 29696
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_SS_RACH_CCCH_Cfg LINE 10
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId[0] = 6
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 8
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 06 02 01 08

- No.: 2055
- Timestamp: 12:21:14:928_0
- RFN: 3258
- Chip: 38144
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB_BCCH_BCH_Cfg LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 246
. . . . . UL_RLC_Mode
. . . . . . UL_TM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . (BooleanType)segmentationIndication = FALSE
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[0] = -
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 1
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_BCCH_Info
- BinaryMessage:
30 1d 02 01 06 02 01 ff 0a 01 00 30 12 30 0b 30 09 02 02 00 f6 30 03 01 01 00 30 03 02 01 01

- No.: 2059
- Timestamp: 12:21:14:936_0
- RFN: 3259
- Chip: 32000
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB_BCCH_BCH_Cfg LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 06 02 01 ff

- No.: 2062
- Timestamp: 12:21:14:938_0
- RFN: 3260
- Chip: 768
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB_PCCH_Cfg LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -2
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 240
. . . . . UL_RLC_Mode
. . . . . . UL_TM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . (BooleanType)segmentationIndication = FALSE
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[0] = -
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 1
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_PCCH_Info
- BinaryMessage:
30 1d 02 01 06 02 01 fe 0a 01 00 30 12 30 0b 30 09 02 02 00 f0 30 03 01 01 00 30 03 02 01 01

- No.: 2066
- Timestamp: 12:21:14:945_0
- RFN: 3260
- Chip: 28928
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB_PCCH_Cfg LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 06 02 01 fe

- No.: 2069
- Timestamp: 12:21:14:947_0
- RFN: 3260
- Chip: 37120
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB0_Cfg LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 0
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 152
. . . . . UL_RLC_Mode
. . . . . . UL_UM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (NoExplicitDiscard)timerBasedNoExplicit[0] = 9
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[0] = -
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 5
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_UM_DL_Info
- BinaryMessage:
30 1d 02 01 06 02 01 00 0a 01 00 30 12 30 0b 30 09 02 02 00 98 30 03 0a 01 09 30 03 02 01 05

- No.: 2073
- Timestamp: 12:21:14:956_0
- RFN: 3261
- Chip: 30976
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB0_Cfg LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 0
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 06 02 01 00

- No.: 2074
- Timestamp: 12:21:14:957_0
- RFN: 3261
- Chip: 37888
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB0_Cfg LINE 3
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 0
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_TM_RLC_Mode
. . . . . . (BooleanType)segmentationIndication = FALSE
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 166
. . . . . UL_RLC_Mode
. . . . . . UL_TM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . (BooleanType)segmentationIndication = FALSE
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 5
. . . . (IntegerType)dLlogicalChannelIdentity[0] = -
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_TM_UL_Info
- BinaryMessage:
30 22 02 01 06 02 01 00 0a 01 00 30 17 30 10 30 03 01 01 00 30 09 02 02 00 a6 30 03 01 01 00 30 03 02 01 05

- No.: 2078
- Timestamp: 12:21:14:966_0
- RFN: 3262
- Chip: 33792
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB0_Cfg LINE 4
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 0
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 06 02 01 00

- No.: 2140
- Timestamp: 12:21:14:982_0
- RFN: 3264
- Chip: 16896
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 10
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 06 02 01 ff 0a 01 00 30 06 02 01 06 02 01 0a

- No.: 2145
- Timestamp: 12:21:14:986_0
- RFN: 3264
- Chip: 32000
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB1_LongNeighCellInfo LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 06 02 01 ff

- No.: 2146
- Timestamp: 12:21:14:987_0
- RFN: 3264
- Chip: 35840
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB1_LongNeighCellInfo LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 1
. . . . . . . (BitStringType)sib_Data_variable[-1] = "1100010000000000000001011000100000001000000000100001000111100000000101111111111111111111111110100101100011011011100110111111111010010101011101010011101001110111111001111010011"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 2
. . . . . . . (BitStringType)sib_Data_variable[-1] = "00000000000000000100"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 24 02 01 06 02 01 ff 00 0e 21 ae c4 00 05 88 08 02 11 e0 17 ff ff fa 58 db 9b fe 95 75 3a 77 e7 a6 21 30 00 04

- No.: 2159
- Timestamp: 12:21:14:992_0
- RFN: 3265
- Chip: 16384
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 10
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 06 02 01 ff 0a 01 00 30 06 02 01 06 02 01 0a

- No.: 2164
- Timestamp: 12:21:14:997_0
- RFN: 3265
- Chip: 37120
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB2_LongNeighCellInfo LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 06 02 01 ff

- No.: 2165
- Timestamp: 12:21:14:998_0
- RFN: 3266
- Chip: 2048
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB2_LongNeighCellInfo LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 1
. . . . . . . (BitStringType)sib_Data_variable[-1] = "1100010000000000000001011000100000001000000000100001000111100000000101111111111111111111111110100101100011011011100110111111111010010101011101010011101001110111111001111010011"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 2
. . . . . . . (BitStringType)sib_Data_variable[-1] = "00000000000000000100"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 24 02 01 06 02 01 ff 00 0e 21 ae c4 00 05 88 08 02 11 e0 17 ff ff fa 58 db 9b fe 95 75 3a 77 e7 a6 21 30 00 04

- No.: 2177
- Timestamp: 12:21:15:001_1
- RFN: 3266
- Chip: 14080
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 7
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 06 02 01 ff 0a 01 00 30 06 02 01 06 02 01 07

- No.: 2182
- Timestamp: 12:21:15:014_0
- RFN: 3267
- Chip: 26880
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB3_LongNeighCellInfo LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 06 02 01 ff

- No.: 2183
- Timestamp: 12:21:15:016_0
- RFN: 3267
- Chip: 34048
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB3_LongNeighCellInfo LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 7
. . . . . . . (BitStringType)sib_Data_variable[-1] = "100000101000000010000001"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 3
. . . . . . . (BitStringType)sib_Data_variable[-1] = "010000000000000000000000000110001011001100011000010000000000001000000100011111111111111111111111"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 1b 02 01 06 02 01 ff 00 0e 27 17 82 80 81 1a fa 00 00 00 c5 98 c2 00 10 23 ff ff f8

- No.: 2195
- Timestamp: 12:21:15:019_3
- RFN: 3268
- Chip: 7424
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 31
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 06 02 01 ff 0a 01 00 30 06 02 01 06 02 01 1f

- No.: 2200
- Timestamp: 12:21:15:034_0
- RFN: 3269
- Chip: 26624
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB4_LongNeighCellInfo LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 06 02 01 ff

- No.: 2201
- Timestamp: 12:21:15:035_0
- RFN: 3269
- Chip: 29952
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB4_LongNeighCellInfo LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 7
. . . . . . . (BitStringType)sib_Data_variable[-1] = "100000101000000010000001"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 4
. . . . . . . (BitStringType)sib_Data_variable[-1] = "0000000000000000000000000011000101100110001100001000000000000100000010001110111"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 19 02 01 06 02 01 ff 00 0e 27 17 82 80 81 22 70 00 00 01 8b 31 84 00 20 47 70

- No.: 2218
- Timestamp: 12:21:15:044_0
- RFN: 3270
- Chip: 24064
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 22
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 06 02 01 ff 0a 01 00 30 06 02 01 06 02 01 16

- No.: 2223
- Timestamp: 12:21:15:046_0
- RFN: 3270
- Chip: 32512
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB5_LongNeighCellInfo LINE 41
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 06 02 01 ff

- No.: 2224
- Timestamp: 12:21:15:047_0
- RFN: 3270
- Chip: 36096
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB5_LongNeighCellInfo LINE 42
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 08 02 01 06 02 01 ff 00 00

- No.: 2228
- Timestamp: 12:21:15:048_0
- RFN: 3271
- Chip: 2048
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 18
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 06 02 01 ff 0a 01 00 30 06 02 01 06 02 01 12

- No.: 2233
- Timestamp: 12:21:15:055_0
- RFN: 3271
- Chip: 31488
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB5_LongNeighCellInfo LINE 44
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 06 02 01 ff

- No.: 2234
- Timestamp: 12:21:15:056_0
- RFN: 3271
- Chip: 34560
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB5_LongNeighCellInfo LINE 45
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . FirstSegment
. . . . . . (SIB_Type)sib_Type[0] = 5
. . . . . . (IntegerType)seg_Count[-1] = 3
. . . . . . (BitStringType)sib_Data_fixed[222] = "000101010100010000111110000000001111111101000011111111111111110111010010000100001111000000101001000011000000101010100101010110000000000000001100110001011011010101111110001010111010000011111110100000111111101000001111111010"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 25 02 01 06 02 01 ff 00 02 52 15 44 3e 00 ff 43 ff fd d2 10 f0 29 0c 0a a5 58 00 0c c5 b5 7e 2b a0 fe 83 fa 0f e8

- No.: 2238
- Timestamp: 12:21:15:057_3
- RFN: 3272
- Chip: 512
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 19
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 06 02 01 ff 0a 01 00 30 06 02 01 06 02 01 13

- No.: 2243
- Timestamp: 12:21:15:075_0
- RFN: 3273
- Chip: 26880
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB5_LongNeighCellInfo LINE 47
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 06 02 01 ff

- No.: 2244
- Timestamp: 12:21:15:076_0
- RFN: 3273
- Chip: 30208
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB5_LongNeighCellInfo LINE 48
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . SubsequentSegment
. . . . . . (SIB_Type)sib_Type[0] = 5
. . . . . . (IntegerType)segmentIndex[-1] = 1
. . . . . . (BitStringType)sib_Data_fixed[222] = "000011111111010000000000000000001101011000110100010000111111010011100101000001100001000011001010000000110000001110001001000000010110000000000000100000001110000000001000100001100100001010011001000010100000000000110000000100"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 25 02 01 06 02 01 ff 00 04 50 0f f4 00 00 d6 34 43 f4 e5 06 10 ca 03 03 89 01 60 00 80 e0 08 86 42 99 0a 00 30 10

- No.: 2248
- Timestamp: 12:21:15:077_2
- RFN: 3273
- Chip: 34560
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 21
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 06 02 01 ff 0a 01 00 30 06 02 01 06 02 01 15

- No.: 2253
- Timestamp: 12:21:15:085_0
- RFN: 3274
- Chip: 24832
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB5_LongNeighCellInfo LINE 50
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 06 02 01 ff

- No.: 2255
- Timestamp: 12:21:15:086_0
- RFN: 3274
- Chip: 28416
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB5_LongNeighCellInfo LINE 52
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . LastSegmentShort
. . . . . . (SIB_Type)sib_Type[0] = 5
. . . . . . (IntegerType)segmentIndex[-1] = 2
. . . . . . (BitStringType)sib_Data_variable[-1] = "010001011100101011010110100000000000011110001000011000000001011011011011011000100000000001000011000010001001010000001011011010000000010000"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 1c 02 01 06 02 01 ff 00 06 51 89 45 ca d6 80 07 88 60 16 db 62 00 43 08 94 0b 68 04 00

- No.: 2272
- Timestamp: 12:21:15:089_1
- RFN: 3275
- Chip: 4096
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 2
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 06 02 01 ff 0a 01 00 30 06 02 01 06 02 01 02

- No.: 2277
- Timestamp: 12:21:15:096_0
- RFN: 3275
- Chip: 32000
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB6_LongNeighCellInfo LINE 8
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 06 02 01 ff

- No.: 2280
- Timestamp: 12:21:15:098_0
- RFN: 3275
- Chip: 36096
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB6_LongNeighCellInfo:lt_CompleteSIB LINE 4
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 6
. . . . . . . (BitStringType)sib_Data_variable[-1] = "0000001010010001"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 0c 02 01 06 02 01 ff 00 0e 06 0f 02 91

- No.: 2285
- Timestamp: 12:21:15:099_0
- RFN: 3276
- Chip: 2048
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 3
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 06 02 01 ff 0a 01 00 30 06 02 01 06 02 01 03

- No.: 2290
- Timestamp: 12:21:15:115_0
- RFN: 3277
- Chip: 26880
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB6_LongNeighCellInfo LINE 11
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 06 02 01 ff

- No.: 2291
- Timestamp: 12:21:15:116_0
- RFN: 3277
- Chip: 29440
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB6_LongNeighCellInfo LINE 12
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 08 02 01 06 02 01 ff 00 00

- No.: 2295
- Timestamp: 12:21:15:117_0
- RFN: 3277
- Chip: 33024
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 5
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 06 02 01 ff 0a 01 00 30 06 02 01 06 02 01 05

- No.: 2300
- Timestamp: 12:21:15:125_0
- RFN: 3278
- Chip: 27904
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB6_LongNeighCellInfo LINE 14
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 06 02 01 ff

- No.: 2301
- Timestamp: 12:21:15:126_0
- RFN: 3278
- Chip: 30464
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB6_LongNeighCellInfo LINE 15
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 08 02 01 06 02 01 ff 00 00

- No.: 2305
- Timestamp: 12:21:15:127_0
- RFN: 3278
- Chip: 34048
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 6
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 06 02 01 ff 0a 01 00 30 06 02 01 06 02 01 06

- No.: 2310
- Timestamp: 12:21:15:144_0
- RFN: 3280
- Chip: 24576
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB6_LongNeighCellInfo LINE 17
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 06 02 01 ff

- No.: 2311
- Timestamp: 12:21:15:145_0
- RFN: 3280
- Chip: 26880
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB6_LongNeighCellInfo LINE 18
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 08 02 01 06 02 01 ff 00 00

- No.: 2319
- Timestamp: 12:21:15:148_3
- RFN: 3281
- Chip: 1280
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 15
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 06 02 01 ff 0a 01 00 30 06 02 01 06 02 01 0f

- No.: 2324
- Timestamp: 12:21:15:164_0
- RFN: 3282
- Chip: 25344
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB7_LongNeighCellInfo LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 06 02 01 ff

- No.: 2328
- Timestamp: 12:21:15:166_0
- RFN: 3282
- Chip: 30464
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB7_LongNeighCellInfo:lt_CompleteSIB7OrLastSIB12_CompleteSIB7 LINE 9
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 7
. . . . . . . (BitStringType)sib_Data_variable[-1] = "100000101000000010000001"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 0d 02 01 06 02 01 ff 00 0e 07 17 82 80 81

- No.: 2336
- Timestamp: 12:21:15:169_0
- RFN: 3283
- Chip: 2560
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 7
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 06 02 01 ff 0a 01 00 30 06 02 01 06 02 01 07

- No.: 2341
- Timestamp: 12:21:15:176_0
- RFN: 3283
- Chip: 31488
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB7_LongNeighCellInfo:lt_ConcatWithSIB3 LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 06 02 01 ff

- No.: 2342
- Timestamp: 12:21:15:177_0
- RFN: 3283
- Chip: 35072
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB7_LongNeighCellInfo:lt_ConcatWithSIB3 LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 7
. . . . . . . (BitStringType)sib_Data_variable[-1] = "100000101000000010000001"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 3
. . . . . . . (BitStringType)sib_Data_variable[-1] = "010000000000000000000000000110001011001100011000010000000000001000000100011111111111111111111111"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 1b 02 01 06 02 01 ff 00 0e 27 17 82 80 81 1a fa 00 00 00 c5 98 c2 00 10 23 ff ff f8

- No.: 2350
- Timestamp: 12:21:15:180_0
- RFN: 3284
- Chip: 7424
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 23
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 06 02 01 ff 0a 01 00 30 06 02 01 06 02 01 17

- No.: 2355
- Timestamp: 12:21:15:186_0
- RFN: 3284
- Chip: 29696
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB7_LongNeighCellInfo:lt_ConcatWithSIB18 LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 06 02 01 ff

- No.: 2356
- Timestamp: 12:21:15:186_1
- RFN: 3284
- Chip: 33024
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB7_LongNeighCellInfo:lt_ConcatWithSIB18 LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 7
. . . . . . . (BitStringType)sib_Data_variable[-1] = "100000101000000010000001"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 26
. . . . . . . (BitStringType)sib_Data_variable[-1] = "100010000111000000000001000000001100000000000100000000110000000000010000000011000000000010000010001"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 1b 02 01 06 02 01 ff 00 0e 27 17 82 80 81 d3 14 43 80 08 06 00 20 18 00 80 60 04 11

- No.: 2364
- Timestamp: 12:21:15:189_1
- RFN: 3285
- Chip: 4864
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 31
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 06 02 01 ff 0a 01 00 30 06 02 01 06 02 01 1f

- No.: 2369
- Timestamp: 12:21:15:204_0
- RFN: 3286
- Chip: 25344
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB7_LongNeighCellInfo:lt_ConcatWithSIB4 LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 06 02 01 ff

- No.: 2370
- Timestamp: 12:21:15:205_0
- RFN: 3286
- Chip: 28416
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB7_LongNeighCellInfo:lt_ConcatWithSIB4 LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 7
. . . . . . . (BitStringType)sib_Data_variable[-1] = "100000101000000010000001"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 4
. . . . . . . (BitStringType)sib_Data_variable[-1] = "0000000000000000000000000011000101100110001100001000000000000100000010001110111"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 19 02 01 06 02 01 ff 00 0e 27 17 82 80 81 22 70 00 00 01 8b 31 84 00 20 47 70

- No.: 2384
- Timestamp: 12:21:15:209_0
- RFN: 3287
- Chip: 4096
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 30
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 06 02 01 ff 0a 01 00 30 06 02 01 06 02 01 1e

- No.: 2389
- Timestamp: 12:21:15:224_0
- RFN: 3288
- Chip: 24832
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB11_LongNeighCellInfo LINE 41
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 06 02 01 ff

- No.: 2390
- Timestamp: 12:21:15:225_0
- RFN: 3288
- Chip: 27392
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB11_LongNeighCellInfo LINE 42
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 08 02 01 06 02 01 ff 00 00

- No.: 2394
- Timestamp: 12:21:15:226_0
- RFN: 3288
- Chip: 31232
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 27
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 06 02 01 ff 0a 01 00 30 06 02 01 06 02 01 1b

- No.: 2399
- Timestamp: 12:21:15:235_0
- RFN: 3289
- Chip: 27136
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB11_LongNeighCellInfo LINE 44
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 06 02 01 ff

- No.: 2400
- Timestamp: 12:21:15:236_0
- RFN: 3289
- Chip: 29952
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB11_LongNeighCellInfo LINE 45
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . SubsequentSegment
. . . . . . (SIB_Type)sib_Type[0] = 11
. . . . . . (IntegerType)segmentIndex[-1] = 1
. . . . . . (BitStringType)sib_Data_fixed[222] = "100001001010100101110000001100101100011011010010100001100101000110010000110110010100011100110100000000010000010010100100101100011011001010001110011010000000001000010001010011001000001101100101000111001101000000000110001101"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 25 02 01 06 02 01 ff 00 04 b0 84 a9 70 32 c6 d2 86 51 90 d9 47 34 01 04 a4 b1 b2 8e 68 02 11 4c 83 65 1c d0 06 34

- No.: 2404
- Timestamp: 12:21:15:237_0
- RFN: 3289
- Chip: 34304
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 26
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 06 02 01 ff 0a 01 00 30 06 02 01 06 02 01 1a

- No.: 2409
- Timestamp: 12:21:15:255_0
- RFN: 3291
- Chip: 27136
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB11_LongNeighCellInfo LINE 47
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 06 02 01 ff

- No.: 2410
- Timestamp: 12:21:15:256_0
- RFN: 3291
- Chip: 30464
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB11_LongNeighCellInfo LINE 48
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . FirstSegment
. . . . . . (SIB_Type)sib_Type[0] = 11
. . . . . . (IntegerType)seg_Count[-1] = 3
. . . . . . (BitStringType)sib_Data_fixed[222] = "001000001101100100000110011000001001001011000100111001010111000010101101100101000111001101000000000000100010001000110010010101010000000100101000010100101010000110000100101000100000101000010000110000100101001001101010100001"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 25 02 01 06 02 01 ff 00 02 b2 20 d9 06 60 92 c4 e5 70 ad 94 73 40 02 22 32 55 01 28 52 a1 84 a2 0a 10 c2 52 6a 84

- No.: 2414
- Timestamp: 12:21:15:257_0
- RFN: 3291
- Chip: 35072
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 29
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 06 02 01 ff 0a 01 00 30 06 02 01 06 02 01 1d

- No.: 2419
- Timestamp: 12:21:15:264_0
- RFN: 3292
- Chip: 24576
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB11_LongNeighCellInfo LINE 50
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 06 02 01 ff

- No.: 2421
- Timestamp: 12:21:15:265_0
- RFN: 3292
- Chip: 27904
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB11_LongNeighCellInfo LINE 52
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . LastSegmentShort
. . . . . . (SIB_Type)sib_Type[0] = 11
. . . . . . (IntegerType)segmentIndex[-1] = 2
. . . . . . (BitStringType)sib_Data_variable[-1] = "100101101111111010010111010100101001100100000110110010100011100110100000000010001000010101001011000011011001010001110011010000000001000101001010101011110001101100101000111001101000000000"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 22 02 01 06 02 01 ff 00 06 b1 b9 96 fe 97 52 99 06 ca 39 a0 08 85 4b 0d 94 73 40 11 4a af 1b 28 e6 80 00

- No.: 2434
- Timestamp: 12:21:15:269_0
- RFN: 3293
- Chip: 3840
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 13
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 06 02 01 ff 0a 01 00 30 06 02 01 06 02 01 0d

- No.: 2439
- Timestamp: 12:21:15:284_0
- RFN: 3294
- Chip: 24576
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB12_LongNeighCellInfo LINE 41
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 06 02 01 ff

- No.: 2440
- Timestamp: 12:21:15:285_0
- RFN: 3294
- Chip: 27392
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB12_LongNeighCellInfo LINE 42
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . SubsequentSegment
. . . . . . (SIB_Type)sib_Type[0] = 12
. . . . . . (IntegerType)segmentIndex[-1] = 1
. . . . . . (BitStringType)sib_Data_fixed[222] = "001100101100011011010010100001100101000110010010110110010100011100110100000000010000010010100100101101011011001010001110011010000000001000010001010011001000101101100101000111001101000000000110001101100101101111111010010111"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 25 02 01 06 02 01 ff 00 04 c0 32 c6 d2 86 51 92 d9 47 34 01 04 a4 b5 b2 8e 68 02 11 4c 8b 65 1c d0 06 36 5b fa 5c

- No.: 2444
- Timestamp: 12:21:15:286_0
- RFN: 3294
- Chip: 31488
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 11
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 06 02 01 ff 0a 01 00 30 06 02 01 06 02 01 0b

- No.: 2449
- Timestamp: 12:21:15:295_0
- RFN: 3295
- Chip: 30208
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB12_LongNeighCellInfo LINE 44
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 06 02 01 ff

- No.: 2450
- Timestamp: 12:21:15:296_0
- RFN: 3295
- Chip: 33536
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB12_LongNeighCellInfo LINE 45
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . FirstSegment
. . . . . . (SIB_Type)sib_Type[0] = 12
. . . . . . (IntegerType)seg_Count[-1] = 3
. . . . . . (BitStringType)sib_Data_fixed[222] = "000000011011001000000100111001010111000010101101100101000111001101000000000000100010001000110010010101010000000100101000010100100000000110000100101000100000101000010000110000100101001001101010100001100001001010100101110000"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 25 02 01 06 02 01 ff 00 02 c2 01 b2 04 e5 70 ad 94 73 40 02 22 32 55 01 28 52 01 84 a2 0a 10 c2 52 6a 86 12 a5 c0

- No.: 2454
- Timestamp: 12:21:15:297_3
- RFN: 3295
- Chip: 37632
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 15
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 06 02 01 ff 0a 01 00 30 06 02 01 06 02 01 0f

- No.: 2459
- Timestamp: 12:21:15:314_0
- RFN: 3297
- Chip: 27136
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB12_LongNeighCellInfo LINE 47
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 06 02 01 ff

- No.: 2464
- Timestamp: 12:21:15:316_2
- RFN: 3297
- Chip: 34560
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB12_LongNeighCellInfo:lt_CompleteSIB7 LINE 7
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 7
. . . . . . . (BitStringType)sib_Data_variable[-1] = "100000101000000010000001"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 0d 02 01 06 02 01 ff 00 0e 07 17 82 80 81

- No.: 2469
- Timestamp: 12:21:15:318_0
- RFN: 3298
- Chip: 768
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 14
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 06 02 01 ff 0a 01 00 30 06 02 01 06 02 01 0e

- No.: 2474
- Timestamp: 12:21:15:335_0
- RFN: 3299
- Chip: 28160
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB12_LongNeighCellInfo LINE 50
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 06 02 01 ff

- No.: 2476
- Timestamp: 12:21:15:337_0
- RFN: 3299
- Chip: 35840
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB12_LongNeighCellInfo LINE 52
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . LastSegmentShort
. . . . . . (SIB_Type)sib_Type[0] = 12
. . . . . . (IntegerType)segmentIndex[-1] = 2
. . . . . . (BitStringType)sib_Data_variable[-1] = "010100101001100100010110110010100011100110100000000010001000010101001011001011011001010001110011010000000001000101001010101011110101101100101000111001101000000000"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 1f 02 01 06 02 01 ff 00 06 c1 a1 52 99 16 ca 39 a0 08 85 4b 2d 94 73 40 11 4a af 5b 28 e6 80 00

- No.: 2484
- Timestamp: 12:21:15:339_3
- RFN: 3300
- Chip: 7680
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 6
. . (IntegerType)sg_POS[-1] = 23
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 06 02 01 ff 0a 01 00 30 06 02 01 06 02 01 17

- No.: 2489
- Timestamp: 12:21:15:354_0
- RFN: 3301
- Chip: 27136
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSIB18_LongNeighCellInfo LINE 5
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 06 02 01 ff

- No.: 2490
- Timestamp: 12:21:15:355_0
- RFN: 3301
- Chip: 30464
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSIB18_LongNeighCellInfo LINE 6
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 7
. . . . . . . (BitStringType)sib_Data_variable[-1] = "100000101000000010000001"
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 26
. . . . . . . (BitStringType)sib_Data_variable[-1] = "100010000111000000000001000000001100000000000100000000110000000000010000000011000000000010000010001"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 1b 02 01 06 02 01 ff 00 0e 27 17 82 80 81 d3 14 43 80 08 06 00 20 18 00 80 60 04 11

- No.: 2502
- Timestamp: 12:21:15:358_1
- RFN: 3302
- Chip: 3584
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 4
. . (IntegerType)sg_POS[-1] = 1
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 06 02 01 ff 0a 01 00 30 06 02 01 04 02 01 01

- No.: 2507
- Timestamp: 12:21:15:365_0
- RFN: 3302
- Chip: 29184
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendSB1_LongNeighCellInfo LINE 4
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 06 02 01 ff

- No.: 2510
- Timestamp: 12:21:15:366_0
- RFN: 3302
- Chip: 33280
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendSB1_LongNeighCellInfo:lt_CompleteSIB LINE 4
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 27
. . . . . . . (BitStringType)sib_Data_variable[-1] = "0001000010101000100000100011000001011101010011100100100110100001000000010101101110010010001011000100010000110010100010010111"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 1a 02 01 06 02 01 ff 00 0e 1b 7b 10 a8 82 30 5d 4e 49 a1 01 5b 92 2c 44 32 89 70

- No.: 2528
- Timestamp: 12:21:15:370_0
- RFN: 3303
- Chip: 9216
- Event: Send
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_REQ
- Source: ts_Scheduling LINE 3
- Message Structure:
CMAC_SYSINFO_Config_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CmacSysinfoConfigReq
. . (IntegerType)sg_REP[-1] = 3
. . (IntegerType)sg_POS[-1] = 0
. . (IntegerType)bcch_ModificationTime[-1] = -
- Constraint:
ca_SchedulNow
- BinaryMessage:
30 11 02 01 06 02 01 ff 0a 01 00 30 06 02 01 03 02 01 00

- No.: 2533
- Timestamp: 12:21:15:375_0
- RFN: 3303
- Chip: 31488
- Event: Receive
- PCO: CMAC
- Message: CMAC_SYSINFO_Config_CNF
- Source: ts_SendMIB LINE 7
- Message Structure:
CMAC_SYSINFO_Config_CNF
. (IntegerType)cellId[0] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_SysInfoCfgCnf
- BinaryMessage:
30 06 02 01 06 02 01 ff

- No.: 2536
- Timestamp: 12:21:15:377_2
- RFN: 3303
- Chip: 35072
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendMIB:lt_CompleteSIB LINE 4
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. tM_message
. . BCCH_BCH_Message
. . . SystemInformation_BCH
. . . . (IntegerType)sfn_Prime[-1] = 0
. . . . payload
. . . . . CompleteSIB_List
. . . . . . CompleteSIBshort
. . . . . . . (SIB_Type)sib_Type[0] = 0
. . . . . . . (BitStringType)sib_Data_variable[-1] = "0001000000000000110001000010010110101010000100010000000000001000100010100000101000100010100001001000100001110001101000100111110010001110010010010010000100000001"
- Constraint:
ca_TR_DataReq
- BinaryMessage:
30 1e 02 01 06 02 01 ff 00 0e 00 9f 10 00 c4 25 aa 11 00 08 8a 0a 22 84 88 71 a2 7c 8e 49 21 01

- No.: 2543
- Timestamp: 12:21:15:379_0
- RFN: 3304
- Chip: 1536
- Event: Start Timer
- Source: ts_RRC_Delay LINE 1
- Message Structure:
no details available
- Constraint:
t_Dly (5000 Ms)
- BinaryMessage:

- No.: 2547
- Timestamp: 12:21:20:373_0
- RFN: 3803
- Chip: 24576
- Event: Timeout
- Source: ts_RRC_Delay LINE 2
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 2559
- Timestamp: 12:21:20:375_0
- RFN: 3803
- Chip: 33024
- Event: Send
- PCO: CMAC
- Message: CMAC_PAGING_Config_REQ
- Source: ts_CMAC_Pag1_Cfg LINE 4
- Message Structure:
CMAC_PAGING_Config_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 5
. (RatType)ratType[0] = 0
. CmacPagingConfigReq
. . pI_BitMapInfo
. . . (BitStringType)e18[18] = '010000000000000000'B
. . (IntegerType)dRX_CycleLength[-1] = 7
. . IMSI_GSM_MAP
. . . (IntegerType)_elem[-1] = 0
. . . (IntegerType)_elem[-1] = 0
. . . (IntegerType)_elem[-1] = 1
. . . (IntegerType)_elem[-1] = 0
. . . (IntegerType)_elem[-1] = 1
. . . (IntegerType)_elem[-1] = 0
. . . (IntegerType)_elem[-1] = 1
. . . (IntegerType)_elem[-1] = 2
. . . (IntegerType)_elem[-1] = 3
. . . (IntegerType)_elem[-1] = 4
. . . (IntegerType)_elem[-1] = 5
. . . (IntegerType)_elem[-1] = 6
. . . (IntegerType)_elem[-1] = 0
. . . (IntegerType)_elem[-1] = 6
. . . (IntegerType)_elem[-1] = 3
. . (BooleanType)t_pich_T_sccpch = FALSE
- Constraint:
ca_CMAC_PagingCfgReq
- BinaryMessage:
30 46 02 01 06 02 01 05 0a 01 00 30 3b 03 04 06 40 40 40 02 01 07 30 2d 02 01 00 02 01 00 02 01 01 02 01 00 02 01 01 02 01 00 02 01 01 02 01 02 02 01 03 02 01 04 02 01 05 02 01 06 02 01 00 02 01 06 02 01 03 01 01 00

- No.: 2563
- Timestamp: 12:21:20:383_0
- RFN: 3804
- Chip: 24832
- Event: Receive
- PCO: CMAC
- Message: CMAC_PAGING_Config_CNF
- Source: ts_CMAC_Pag1_Cfg LINE 5
- Message Structure:
CMAC_PAGING_Config_CNF
. (IntegerType)cellId[0] = 6
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 5
- Constraint:
ca_CMAC_PagingCfgCnf
- BinaryMessage:
30 06 02 01 06 02 01 05

- No.: 2565
- Timestamp: 12:21:20:384_0
- RFN: 3804
- Chip: 27904
- Event: Send
- PCO: TM
- Message: RLC_TR_DATA_REQ
- Source: ts_SendPage1_ModifySI LINE 3
- Message Structure:
RLC_TR_DATA_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -2
. tM_message
. . PCCH_Message
. . . PCCH_MessageType
. . . . PagingType1
. . . . . PagingRecordList
. . . . . BCCH_ModificationInfo
. . . . . . (IntegerType)mib_ValueTag[-1] = 2
. . . . . . (IntegerType)bcch_ModificationTime[-1] = -
. . . . . laterNonCriticalExtensions
- Constraint:
cas_PagingType1
- BinaryMessage:
30 07 02 01 06 02 01 fe 21

- No.: 2595
- Timestamp: 12:21:20:403_0
- RFN: 3806
- Chip: 21760
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_ReconfigFACH_ToNoDedicated LINE 3
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 5
. (RatType)ratType[0] = 0
. configMessage
. . CmacConfigReq
. . . SS_ActivationTime
. . . UE_Info
. . . . U_RNTI
. . . . (BitStringType)c_RNTI[16] = -
. . . TrCHInfo
. . . . ulconnectedTrCHList
. . . . TFCS
. . . . dlconnectedTrCHList
. . . . . TrCHInfo_setseq_1
. . . . . . (IntegerType)trchid[-1] = 12
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size[-1] = 240
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional[0] = 0
. . . . . . . . (IntegerType)rateMatchingAttribute[-1] = 230
. . . . . . . . (CRC_Size)crc_Size[0] = 3
. . . . . TrCHInfo_setseq_1
. . . . . . (IntegerType)trchid[-1] = 13
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size[-1] = 168
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . (IntegerType)small[-1] = 2
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional[0] = 0
. . . . . . . . (IntegerType)rateMatchingAttribute[-1] = 220
. . . . . . . . (CRC_Size)crc_Size[0] = 3
. . . . . TrCHInfo_setseq_1
. . . . . . (IntegerType)trchid[-1] = 14
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size[-1] = 360
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . (IntegerType)rateMatchingAttribute[-1] = 130
. . . . . . . . (CRC_Size)crc_Size[0] = 3
. . . . TFCS
. . . . . ExplicitTFCS_Configuration
. . . . . . TFCS_ReconfAdd
. . . . . . . ctfcSize
. . . . . . . . ctfc4Bit
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4[-1] = 0
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4[-1] = 1
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4[-1] = 2
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4[-1] = 3
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4[-1] = 4
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4[-1] = 5
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4[-1] = 6
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4[-1] = 8
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC[-1] = 11
. . . . . . . . . . . . . (IntegerType)gainFactorBetaD[-1] = 15
. . . . . . . . . . . . . (IntegerType)referenceTFC_ID[-1] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . TrCH_LogCHMappingList1
. . . . ulconnectedTrCHList
. . . . dlconnectedTrCHList
. . . . . TrCH_LogCHMappingList1_setseq_1
. . . . . . (IntegerType)trchid[-1] = 12
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation[0] = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType[0] = 3
. . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . . . (LogicalChannelType)logicalChannelType[0] = 1
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 1
. . . . . . . . (IntegerType)rB_Identity[-1] = -2
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
. . . . . TrCH_LogCHMappingList1_setseq_1
. . . . . . (IntegerType)trchid[-1] = 13
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation[0] = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType[0] = 1
. . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 5
. . . . . . . . . . (LogicalChannelType)logicalChannelType[0] = 2
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 1
. . . . . . . . (IntegerType)rB_Identity[-1] = 0
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_CMAC_ReconfigInfoActNow
- BinaryMessage:
30 82 01 21 02 01 00 02 01 05 0a 01 00 30 82 01 14 05 00 30 00 30 81 cb 30 6b 30 21 02 01 0c 30 1c 30 0e 30 0c 02 02 00 f0 30 04 05 00 05 00 05 00 30 0a 0a 01 00 02 02 00 e6 0a 01 03 30 24 02 01 0d 30 1f 30 11 30 0f 02 02 00 a8 30 07 05 00 05 00 02 01 02 05 00 30 0a 0a 01 00 02 02 00 dc 0a 01 03 30 20 02 01 0e 30 1b 30 0e 30 0c 02 02 01 68 30 04 05 00 05 00 05 00 30 09 05 00 02 02 00 82 0a 01 03 30 5c 30 5a 30 08 02 01 00 30 03 02 01 00 30 08 02 01 01 30 03 02 01 00 30 08 02 01 02 30 03 02 01 00 30 08 02 01 03 30 03 02 01 00 30 08 02 01 04 30 03 02 01 00 30 08 02 01 05 30 03 02 01 00 30 08 02 01 06 30 03 02 01 00 30 12 02 01 08 30 0d 30 0b 30 03 02 01 0b 02 01 0f 02 01 00 30 40 30 3e 30 1d 02 01 0c 30 18 30 16 30 11 0a 01 00 0a 01 03 02 01 01 0a 01 01 05 00 02 01 01 02 01 fe 30 1d 02 01 0d 30 18 30 16 30 11 0a 01 00 0a 01 01 02 01 05 0a 01 02 05 00 02 01 01 02 01 00

- No.: 2596
- Timestamp: 12:21:20:409_0
- RFN: 3807
- Chip: 4864
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_ReconfigFACH_ToNoDedicated LINE 4
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 5
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 05

- No.: 2597
- Timestamp: 12:21:20:416_0
- RFN: 3807
- Chip: 32512
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_ReconfigFACH_ToNoDedicated LINE 5
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 8
. (RatType)ratType[0] = 0
. configMessage
. . CmacConfigReq
. . . SS_ActivationTime
. . . UE_Info
. . . . U_RNTI
. . . . (BitStringType)c_RNTI[16] = -
. . . TrCHInfo
. . . . ulconnectedTrCHList
. . . . . TrCHInfo_setseq_0
. . . . . . (IntegerType)trchid[-1] = 15
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size[-1] = 168
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size[-1] = 360
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional[0] = 0
. . . . . . . . (IntegerType)rateMatchingAttribute[-1] = 150
. . . . . . . . (CRC_Size)crc_Size[0] = 3
. . . . TFCS
. . . . . ExplicitTFCS_Configuration
. . . . . . TFCS_ReconfAdd
. . . . . . . ctfcSize
. . . . . . . . ctfc2Bit
. . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . (IntegerType)ctfc2[-1] = 0
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . (IntegerType)ctfc2[-1] = 1
. . . . . . . . . . PowerOffsetInformation
. . . . dlconnectedTrCHList
. . . . TFCS
. . . TrCH_LogCHMappingList1
. . . . ulconnectedTrCHList
. . . . . TrCH_LogCHMappingList1_setseq_0
. . . . . . (IntegerType)trchid[-1] = 15
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation[0] = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType[0] = 1
. . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 5
. . . . . . . . . . (LogicalChannelType)logicalChannelType[0] = 2
. . . . . . . . (IntegerType)rB_Identity[-1] = 0
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
. . . . dlconnectedTrCHList
- Constraint:
ca_CMAC_ReconfigInfoActNow
- BinaryMessage:
30 6c 02 01 00 02 01 08 0a 01 00 30 61 05 00 30 00 30 3d 30 2d 30 2b 02 01 0f 30 26 30 18 30 0a 02 02 00 a8 30 02 05 00 05 00 30 0a 02 02 01 68 30 02 05 00 05 00 30 0a 0a 01 00 02 02 00 96 0a 01 03 30 0c 30 0a 30 03 02 01 00 30 03 02 01 01 30 1c 30 1a 30 18 02 01 0f 30 13 30 11 30 0c 0a 01 00 0a 01 01 02 01 05 0a 01 02 02 01 00

- No.: 2604
- Timestamp: 12:21:20:423_0
- RFN: 3808
- Chip: 19456
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_ReconfigFACH_ToNoDedicated LINE 6
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 8
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 08

- No.: 2608
- Timestamp: 12:21:20:424_0
- RFN: 3808
- Chip: 26112
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -3
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 00 02 01 fd 0a 01 00 05 00

- No.: 2612
- Timestamp: 12:21:20:427_0
- RFN: 3808
- Chip: 36352
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -3
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 fd

- No.: 2624
- Timestamp: 12:21:20:443_0
- RFN: 3810
- Chip: 20736
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_SS_ReconfNoDedicatedToCellFACH LINE 3
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 5
. (RatType)ratType[0] = 0
. configMessage
. . CmacConfigReq
. . . SS_ActivationTime
. . . UE_Info
. . . . U_RNTI
. . . . . (BitStringType)srnc_Identity[12] = "000000000001"
. . . . . (BitStringType)s_RNTI[20] = "00000000000000000001"
. . . . (BitStringType)c_RNTI[16] = "0000000000000001"
. . . TrCHInfo
. . . . ulconnectedTrCHList
. . . . TFCS
. . . . dlconnectedTrCHList
. . . . . TrCHInfo_setseq_1
. . . . . . (IntegerType)trchid[-1] = 12
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size[-1] = 240
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional[0] = 0
. . . . . . . . (IntegerType)rateMatchingAttribute[-1] = 230
. . . . . . . . (CRC_Size)crc_Size[0] = 3
. . . . . TrCHInfo_setseq_1
. . . . . . (IntegerType)trchid[-1] = 13
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size[-1] = 168
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . (IntegerType)small[-1] = 2
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional[0] = 0
. . . . . . . . (IntegerType)rateMatchingAttribute[-1] = 220
. . . . . . . . (CRC_Size)crc_Size[0] = 3
. . . . . TrCHInfo_setseq_1
. . . . . . (IntegerType)trchid[-1] = 14
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size[-1] = 360
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . (IntegerType)rateMatchingAttribute[-1] = 130
. . . . . . . . (CRC_Size)crc_Size[0] = 3
. . . . TFCS
. . . . . ExplicitTFCS_Configuration
. . . . . . TFCS_ReconfAdd
. . . . . . . ctfcSize
. . . . . . . . ctfc4Bit
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4[-1] = 0
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4[-1] = 1
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4[-1] = 2
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4[-1] = 3
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4[-1] = 4
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4[-1] = 5
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4[-1] = 6
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . . . TFCS_ReconfAdd_setseq_1
. . . . . . . . . . (IntegerType)ctfc4[-1] = 8
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC[-1] = 11
. . . . . . . . . . . . . (IntegerType)gainFactorBetaD[-1] = 15
. . . . . . . . . . . . . (IntegerType)referenceTFC_ID[-1] = 0
. . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . TrCH_LogCHMappingList1
. . . . ulconnectedTrCHList
. . . . dlconnectedTrCHList
. . . . . TrCH_LogCHMappingList1_setseq_1
. . . . . . (IntegerType)trchid[-1] = 12
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation[0] = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType[0] = 3
. . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . . . (LogicalChannelType)logicalChannelType[0] = 1
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 1
. . . . . . . . (IntegerType)rB_Identity[-1] = -2
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
. . . . . TrCH_LogCHMappingList1_setseq_1
. . . . . . (IntegerType)trchid[-1] = 13
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation[0] = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType[0] = 1
. . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 6
. . . . . . . . . . (LogicalChannelType)logicalChannelType[0] = 0
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 6
. . . . . . . . (IntegerType)rB_Identity[-1] = -3
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation[0] = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType[0] = 1
. . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 5
. . . . . . . . . . (LogicalChannelType)logicalChannelType[0] = 2
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 1
. . . . . . . . (IntegerType)rB_Identity[-1] = 0
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation[0] = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType[0] = 1
. . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . . . (LogicalChannelType)logicalChannelType[0] = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 1
. . . . . . . . (IntegerType)rB_Identity[-1] = 1
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation[0] = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType[0] = 1
. . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 2
. . . . . . . . . . (LogicalChannelType)logicalChannelType[0] = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 2
. . . . . . . . (IntegerType)rB_Identity[-1] = 2
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation[0] = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType[0] = 1
. . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 3
. . . . . . . . . . (LogicalChannelType)logicalChannelType[0] = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 3
. . . . . . . . (IntegerType)rB_Identity[-1] = 3
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation[0] = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType[0] = 1
. . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 4
. . . . . . . . . . (LogicalChannelType)logicalChannelType[0] = 4
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 4
. . . . . . . . (IntegerType)rB_Identity[-1] = 4
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
. . . . . TrCH_LogCHMappingList1_setseq_1
. . . . . . (IntegerType)trchid[-1] = 14
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_DL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation[0] = 0
. . . . . . . . . . (SS_DL_TransportChannelType)dl_TransportChannelType[0] = 1
. . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 7
. . . . . . . . . . (LogicalChannelType)logicalChannelType[0] = 5
. . . . . . . . . . rlc_SizeList
. . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 8
. . . . . . . . (IntegerType)rB_Identity[-1] = 20
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_CMAC_ReconfigInfoActNow
- BinaryMessage:
30 82 01 ce 02 01 06 02 01 05 0a 01 00 30 82 01 c1 05 00 30 12 30 0b 03 03 04 00 00 03 04 04 00 00 00 03 03 00 00 00 30 81 cb 30 6b 30 21 02 01 0c 30 1c 30 0e 30 0c 02 02 00 f0 30 04 05 00 05 00 05 00 30 0a 0a 01 00 02 02 00 e6 0a 01 03 30 24 02 01 0d 30 1f 30 11 30 0f 02 02 00 a8 30 07 05 00 05 00 02 01 02 05 00 30 0a 0a 01 00 02 02 00 dc 0a 01 03 30 20 02 01 0e 30 1b 30 0e 30 0c 02 02 01 68 30 04 05 00 05 00 05 00 30 09 05 00 02 02 00 82 0a 01 03 30 5c 30 5a 30 08 02 01 00 30 03 02 01 00 30 08 02 01 01 30 03 02 01 00 30 08 02 01 02 30 03 02 01 00 30 08 02 01 03 30 03 02 01 00 30 08 02 01 04 30 03 02 01 00 30 08 02 01 05 30 03 02 01 00 30 08 02 01 06 30 03 02 01 00 30 12 02 01 08 30 0d 30 0b 30 03 02 01 0b 02 01 0f 02 01 00 30 81 da 30 81 d7 30 1d 02 01 0c 30 18 30 16 30 11 0a 01 00 0a 01 03 02 01 01 0a 01 01 05 00 02 01 01 02 01 fe 30 81 96 02 01 0d 30 81 90 30 16 30 11 0a 01 00 0a 01 01 02 01 06 0a 01 00 05 00 02 01 06 02 01 fd 30 16 30 11 0a 01 00 0a 01 01 02 01 05 0a 01 02 05 00 02 01 01 02 01 00 30 16 30 11 0a 01 00 0a 01 01 02 01 01 0a 01 04 05 00 02 01 01 02 01 01 30 16 30 11 0a 01 00 0a 01 01 02 01 02 0a 01 04 05 00 02 01 02 02 01 02 30 16 30 11 0a 01 00 0a 01 01 02 01 03 0a 01 04 05 00 02 01 03 02 01 03 30 16 30 11 0a 01 00 0a 01 01 02 01 04 0a 01 04 05 00 02 01 04 02 01 04 30 1d 02 01 0e 30 18 30 16 30 11 0a 01 00 0a 01 01 02 01 07 0a 01 05 05 00 02 01 08 02 01 14

- No.: 2628
- Timestamp: 12:21:20:454_0
- RFN: 3811
- Chip: 25344
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_SS_ReconfNoDedicatedToCellFACH LINE 4
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId[0] = 6
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 5
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 06 02 01 05

- No.: 2629
- Timestamp: 12:21:20:459_0
- RFN: 3812
- Chip: 6656
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_SS_ReconfNoDedicatedToCellFACH LINE 5
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 8
. (RatType)ratType[0] = 0
. configMessage
. . CmacConfigReq
. . . SS_ActivationTime
. . . UE_Info
. . . . U_RNTI
. . . . (BitStringType)c_RNTI[16] = "0000000000000001"
. . . TrCHInfo
. . . . ulconnectedTrCHList
. . . . . TrCHInfo_setseq_0
. . . . . . (IntegerType)trchid[-1] = 15
. . . . . . CommonOrDedicatedTFS
. . . . . . . tti
. . . . . . . . CommonOrDedicatedTF_InfoList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size[-1] = 168
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . . . CommonOrDedicatedTF_Info
. . . . . . . . . . (IntegerType)tb_Size[-1] = 360
. . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . LogicalChannelList
. . . . . . . SemistaticTF_Information
. . . . . . . . ChannelCodingType
. . . . . . . . . (CodingRate)convolutional[0] = 0
. . . . . . . . (IntegerType)rateMatchingAttribute[-1] = 150
. . . . . . . . (CRC_Size)crc_Size[0] = 3
. . . . TFCS
. . . . . ExplicitTFCS_Configuration
. . . . . . TFCS_ReconfAdd
. . . . . . . ctfcSize
. . . . . . . . ctfc2Bit
. . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . (IntegerType)ctfc2[-1] = 0
. . . . . . . . . . PowerOffsetInformation
. . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . (IntegerType)ctfc2[-1] = 1
. . . . . . . . . . PowerOffsetInformation
. . . . dlconnectedTrCHList
. . . . TFCS
. . . TrCH_LogCHMappingList1
. . . . ulconnectedTrCHList
. . . . . TrCH_LogCHMappingList1_setseq_0
. . . . . . (IntegerType)trchid[-1] = 15
. . . . . . TrCH_LogCHMappingList
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation[0] = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType[0] = 1
. . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 5
. . . . . . . . . . (LogicalChannelType)logicalChannelType[0] = 2
. . . . . . . . (IntegerType)rB_Identity[-1] = 0
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation[0] = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType[0] = 1
. . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . . . (LogicalChannelType)logicalChannelType[0] = 4
. . . . . . . . (IntegerType)rB_Identity[-1] = 1
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation[0] = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType[0] = 1
. . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 2
. . . . . . . . . . (LogicalChannelType)logicalChannelType[0] = 4
. . . . . . . . (IntegerType)rB_Identity[-1] = 2
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation[0] = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType[0] = 1
. . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 3
. . . . . . . . . . (LogicalChannelType)logicalChannelType[0] = 4
. . . . . . . . (IntegerType)rB_Identity[-1] = 3
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation[0] = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType[0] = 1
. . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 4
. . . . . . . . . . (LogicalChannelType)logicalChannelType[0] = 4
. . . . . . . . (IntegerType)rB_Identity[-1] = 4
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
. . . . . . . TrCH_LogicalChannelMapping
. . . . . . . . logicalChannel_Mapping
. . . . . . . . . SS_UL_LogicalChannelMapping
. . . . . . . . . . (MAC_HeaderManipulation)macHeaderManipulation[0] = 0
. . . . . . . . . . (SS_UL_TransportChannelType)ul_TransportChannelType[0] = 1
. . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 7
. . . . . . . . . . (LogicalChannelType)logicalChannelType[0] = 5
. . . . . . . . (IntegerType)rB_Identity[-1] = 20
. . . . . . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
. . . . dlconnectedTrCHList
- Constraint:
ca_CMAC_ReconfigInfoActNow
- BinaryMessage:
30 81 d1 02 01 06 02 01 08 0a 01 00 30 81 c5 05 00 30 05 03 03 00 00 00 30 3d 30 2d 30 2b 02 01 0f 30 26 30 18 30 0a 02 02 00 a8 30 02 05 00 05 00 30 0a 02 02 01 68 30 02 05 00 05 00 30 0a 0a 01 00 02 02 00 96 0a 01 03 30 0c 30 0a 30 03 02 01 00 30 03 02 01 01 30 7b 30 79 30 77 02 01 0f 30 72 30 11 30 0c 0a 01 00 0a 01 01 02 01 05 0a 01 02 02 01 00 30 11 30 0c 0a 01 00 0a 01 01 02 01 01 0a 01 04 02 01 01 30 11 30 0c 0a 01 00 0a 01 01 02 01 02 0a 01 04 02 01 02 30 11 30 0c 0a 01 00 0a 01 01 02 01 03 0a 01 04 02 01 03 30 11 30 0c 0a 01 00 0a 01 01 02 01 04 0a 01 04 02 01 04 30 11 30 0c 0a 01 00 0a 01 01 02 01 07 0a 01 05 02 01 14

- No.: 2633
- Timestamp: 12:21:20:465_0
- RFN: 3812
- Chip: 29696
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_SS_ReconfNoDedicatedToCellFACH LINE 6
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId[0] = 6
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 8
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 06 02 01 08

- No.: 2637
- Timestamp: 12:21:20:468_0
- RFN: 3813
- Chip: 3072
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB_BCCH_FACH_Cfg LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -3
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 166
. . . . . UL_RLC_Mode
. . . . . . UL_TM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . (BooleanType)segmentationIndication = TRUE
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[0] = -
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 6
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_TM_DL_Info
- BinaryMessage:
30 1d 02 01 06 02 01 fd 0a 01 00 30 12 30 0b 30 09 02 02 00 a6 30 03 01 01 ff 30 03 02 01 06

- No.: 2641
- Timestamp: 12:21:20:475_0
- RFN: 3813
- Chip: 29696
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB_BCCH_FACH_Cfg LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -3
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 06 02 01 fd

- No.: 2666
- Timestamp: 12:21:21:686_0
- RFN: 3934
- Chip: 34304
- Event: Receive
- PCO: TM
- Message: RLC_TR_DATA_IND
- Source: ts_RRC_ConnEst:lt_RcvConnReq LINE 2
- Message Structure:
RLC_TR_DATA_IND
. (IntegerType)cellId[0] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 0
. tM_message
. . UL_CCCH_Message
. . . IntegrityCheckInfo
. . . UL_CCCH_MessageType
. . . . RRCConnectionRequest
. . . . . InitialUE_Identity
. . . . . . TMSI_and_LAI_GSM_MAP
. . . . . . . (BitStringType)tmsi[32] = "00010010001101000101011001111000"
. . . . . . . LAI
. . . . . . . . PLMN_Identity
. . . . . . . . . MCC
. . . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . . (IntegerType)_elem[4] = 1
. . . . . . . . . MNC
. . . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . . (IntegerType)_elem[4] = 1
. . . . . . . . (BitStringType)lac[16] = '0000000000000001'B
. . . . . (EstablishmentCause)establishmentCause[5] = 12
. . . . . (ProtocolErrorIndicator)protocolErrorIndicator[1] = 0
. . . . . MeasuredResultsOnRACH
. . . . . v3d0NonCriticalExtensions
- Constraint:
car_RRC_ConnReq
- BinaryMessage:
30 11 02 01 06 02 01 00 21 12 34 56 78 00 10 08 00 0b 00

- No.: 2670
- Timestamp: 12:21:21:696_0
- RFN: 3935
- Chip: 33536
- Event: Send
- PCO: UM
- Message: RLC_UM_DATA_REQ
- Source: ts_RRC_ConnEst:lt_Send_ConnSetUp LINE 2
- Message Structure:
RLC_UM_DATA_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 0
. uM_message
. . DL_CCCH_Message
. . . IntegrityCheckInfo
. . . DL_CCCH_MessageType
. . . . RRCConnectionSetup
. . . . . r3
. . . . . . RRCConnectionSetup_r3_IEs
. . . . . . . InitialUE_Identity
. . . . . . . . TMSI_and_LAI_GSM_MAP
. . . . . . . . . (BitStringType)tmsi[32] = "00010010001101000101011001111000"
. . . . . . . . . LAI
. . . . . . . . . . PLMN_Identity
. . . . . . . . . . . MCC
. . . . . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . . . . (IntegerType)_elem[4] = 1
. . . . . . . . . . . MNC
. . . . . . . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . . . . . . (IntegerType)_elem[4] = 1
. . . . . . . . . . (BitStringType)lac[16] = '0000000000000001'B
. . . . . . . (IntegerType)rrc_TransactionIdentifier[-1] = 0
. . . . . . . (IntegerType)activationTime[-1] = -
. . . . . . . U_RNTI
. . . . . . . . (BitStringType)srnc_Identity[12] = "000000000001"
. . . . . . . . (BitStringType)s_RNTI[20] = "00000000000000000001"
. . . . . . . (BitStringType)new_c_RNTI[16] = "0000000000000001"
. . . . . . . (RRC_StateIndicator)rrc_StateIndicator[0] = 1
. . . . . . . (IntegerType)utran_DRX_CycleLengthCoeff[-1] = 9
. . . . . . . CapabilityUpdateRequirement
. . . . . . . . (BooleanType)ue_RadioCapabilityFDDUpdateRequirement = TRUE
. . . . . . . . (BooleanType)ue_RadioCapabilityTDDUpdateRequirement = FALSE
. . . . . . . . SystemSpecificCapUpdateReqList
. . . . . . . . . (SystemSpecificCapUpdateReq)_elem[0] = 0
. . . . . . . SRB_InformationSetupList2
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity[-1] = 1
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_UM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (NoExplicitDiscard)timerBasedNoExplicit[0] = 4
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex[-1] = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 1
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 1
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 1
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity[-1] = 2
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 2
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex[-1] = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 2
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 2
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 2
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 2
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 2
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity[-1] = 3
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 3
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex[-1] = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 3
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 3
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 3
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 3
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 3
. . . . . . . . SRB_InformationSetup
. . . . . . . . . (IntegerType)rb_Identity[-1] = 4
. . . . . . . . . RLC_InfoChoice
. . . . . . . . . . RLC_Info
. . . . . . . . . . . UL_RLC_Mode
. . . . . . . . . . . . UL_AM_RLC_Mode
. . . . . . . . . . . . . TransmissionRLC_Discard
. . . . . . . . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . . . . . . . PollingInfo
. . . . . . . . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . . . . . . . . . DL_RLC_Mode
. . . . . . . . . . . . DL_AM_RLC_Mode
. . . . . . . . . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . . . . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . . . . . . . . DL_RLC_StatusInfo
. . . . . . . . . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . . . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . . . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . . . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . . . . . . RB_MappingInfo
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 4
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . . RLC_SizeExplicitList
. . . . . . . . . . . . . . . RLC_SizeInfo
. . . . . . . . . . . . . . . . (IntegerType)rlc_SizeIndex[-1] = 1
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 4
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 4
. . . . . . . . . . RB_MappingOption
. . . . . . . . . . . UL_LogicalChannelMappings
. . . . . . . . . . . . UL_LogicalChannelMapping
. . . . . . . . . . . . . UL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 5
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 4
. . . . . . . . . . . . . rlc_SizeList
. . . . . . . . . . . . . (IntegerType)mac_LogicalChannelPriority[-1] = 4
. . . . . . . . . . . DL_LogicalChannelMappingList
. . . . . . . . . . . . DL_LogicalChannelMapping
. . . . . . . . . . . . . DL_TransportChannelType
. . . . . . . . . . . . . . (IntegerType)dch[-1] = 10
. . . . . . . . . . . . . (IntegerType)logicalChannelIdentity[-1] = 4
. . . . . . . UL_CommonTransChInfo
. . . . . . . . TFC_Subset
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . TFCS
. . . . . . . . . . . ExplicitTFCS_Configuration
. . . . . . . . . . . . TFCS_ReconfAdd
. . . . . . . . . . . . . ctfcSize
. . . . . . . . . . . . . . ctfc2Bit
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . . . . . . . (IntegerType)ctfc2[-1] = 0
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . (IntegerType)computedGainFactors[-1] = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . . . . . . . . . TFCS_ReconfAdd_setseq_0
. . . . . . . . . . . . . . . . (IntegerType)ctfc2[-1] = 1
. . . . . . . . . . . . . . . . PowerOffsetInformation
. . . . . . . . . . . . . . . . . GainFactorInformation
. . . . . . . . . . . . . . . . . . SignalledGainFactors
. . . . . . . . . . . . . . . . . . . modeSpecificInfo
. . . . . . . . . . . . . . . . . . . . fdd
. . . . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaC[-1] = 11
. . . . . . . . . . . . . . . . . . . (IntegerType)gainFactorBetaD[-1] = 15
. . . . . . . . . . . . . . . . . . . (IntegerType)referenceTFC_ID[-1] = 0
. . . . . . . . . . . . . . . . . (IntegerType)powerOffsetPp_m[-1] = -
. . . . . . . UL_AddReconfTransChInfoList
. . . . . . . . UL_AddReconfTransChInformation
. . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType[0] = 0
. . . . . . . . . (IntegerType)transportChannelIdentity[-1] = 5
. . . . . . . . . TransportFormatSet
. . . . . . . . . . DedicatedTransChTFS
. . . . . . . . . . . tti
. . . . . . . . . . . . DedicatedDynamicTF_InfoList
. . . . . . . . . . . . . DedicatedDynamicTF_Info
. . . . . . . . . . . . . . rlc_Size
. . . . . . . . . . . . . . . BitModeRLC_SizeInfo
. . . . . . . . . . . . . . . . sizeType2
. . . . . . . . . . . . . . . . . (IntegerType)part1[-1] = 2
. . . . . . . . . . . . . . . . . (IntegerType)part2[-1] = -
. . . . . . . . . . . . . . numberOfTbSizeList
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . . NumberOfTransportBlocks
. . . . . . . . . . . . . . LogicalChannelList
. . . . . . . . . . . SemistaticTF_Information
. . . . . . . . . . . . ChannelCodingType
. . . . . . . . . . . . . (CodingRate)convolutional[0] = 1
. . . . . . . . . . . . (IntegerType)rateMatchingAttribute[-1] = 170
. . . . . . . . . . . . (CRC_Size)crc_Size[0] = 3
. . . . . . . DL_CommonTransChInfo
. . . . . . . . TFCS
. . . . . . . . modeSpecificInfo
. . . . . . . . . fdd
. . . . . . . . . . dl_Parameters
. . . . . . . DL_AddReconfTransChInfoList
. . . . . . . . DL_AddReconfTransChInformation
. . . . . . . . . (DL_TrCH_Type)dl_TransportChannelType[0] = 0
. . . . . . . . . (IntegerType)dl_transportChannelIdentity[-1] = 10
. . . . . . . . . tfs_SignallingMode
. . . . . . . . . . UL_TransportChannelIdentity
. . . . . . . . . . . (UL_TrCH_Type)ul_TransportChannelType[0] = 0
. . . . . . . . . . . (IntegerType)ul_TransportChannelIdentity[-1] = 5
. . . . . . . . . QualityTarget
. . . . . . . . . . (IntegerType)bler_QualityValue[-1] = -20
. . . . . . . . . TM_SignallingInfo
. . . . . . . FrequencyInfo
. . . . . . . (IntegerType)maxAllowedUL_TX_Power[-1] = -
. . . . . . . UL_ChannelRequirement
. . . . . . . DL_CommonInformation
. . . . . . . DL_InformationPerRL_List
. . . . . . laterNonCriticalExtensions
. (BooleanType)specialLI = TRUE
- Constraint:
cas_RRC_ConnSetup
- BinaryMessage:
30 6c 02 01 06 02 01 00 31 e0 22 46 8a cf 00 02 01 00 01 00 04 00 00 40 00 5d 83 03 6a 27 50 80 00 a1 a1 01 08 90 85 9e 8e 46 c9 a6 7c 9c 4e 75 18 00 2a 3a 10 52 89 18 99 e8 e4 6c 9a 67 c9 c4 e7 52 80 04 a5 a1 09 48 92 8d 9e 8e 46 c9 a6 7c 9c 4e 75 38 00 6a 7a 10 d6 89 32 00 01 89 4a fc 00 84 02 20 88 ea 59 82 26 25 60 01 01 ff

- No.: 2691
- Timestamp: 12:21:21:718_1
- RFN: 3938
- Chip: 1536
- Event: Start Timer
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 8
- Message Structure:
no details available
- Constraint:
t_WaitMS (13500 Ms)
- BinaryMessage:

- No.: 2697
- Timestamp: 12:21:22:086_0
- RFN: 3974
- Chip: 34048
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_IND
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 10
- Message Structure:
RLC_AM_DATA_IND
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
. IntegrityResult
. . (IntegrityStatus)integrityUsed[0] = 4294967296
. aM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . UL_DCCH_MessageType
. . . . RRCConnectionSetupComplete
. . . . . (IntegerType)rrc_TransactionIdentifier[2] = 0
. . . . . STARTList
. . . . . . STARTSingle
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity[1] = 0
. . . . . . . (BitStringType)start_Value[20] = "00000000000000000010"
. . . . . . STARTSingle
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity[1] = 1
. . . . . . . (BitStringType)start_Value[20] = "00000000000000000010"
. . . . . UE_RadioAccessCapability
. . . . . . (AccessStratumReleaseIndicator)accessStratumReleaseIndicator[0] = 0
. . . . . . PDCP_Capability
. . . . . . . (BooleanType)losslessSRNS_RelocationSupport = FALSE
. . . . . . . supportForRfc2507
. . . . . . RLC_Capability
. . . . . . . (TotalRLC_AM_BufferSize)totalRLC_AM_BufferSize[3] = 2
. . . . . . . (MaximumRLC_WindowSize)maximumRLC_WindowSize[1] = 0
. . . . . . . (MaximumAM_EntityNumberRLC_Cap)maximumAM_EntityNumber[3] = 3
. . . . . . TransportChannelCapability
. . . . . . . DL_TransChCapability
. . . . . . . . (MaxNoBits)maxNoBitsReceived[4] = 5
. . . . . . . . (MaxNoBits)maxConvCodeBitsReceived[4] = 0
. . . . . . . . TurboSupport
. . . . . . . . . (MaxNoBits)supported[4] = 5
. . . . . . . . (MaxSimultaneousTransChsDL)maxSimultaneousTransChs[2] = 1
. . . . . . . . (IntegerType)maxSimultaneousCCTrCH_Count[3] = 1
. . . . . . . . (MaxTransportBlocksDL)maxReceivedTransportBlocks[4] = 3
. . . . . . . . (MaxNumberOfTFC_DL)maxNumberOfTFC[4] = 5
. . . . . . . . (MaxNumberOfTF)maxNumberOfTF[3] = 1
. . . . . . . UL_TransChCapability
. . . . . . . . (MaxNoBits)maxNoBitsTransmitted[4] = 3
. . . . . . . . (MaxNoBits)maxConvCodeBitsTransmitted[4] = 0
. . . . . . . . TurboSupport
. . . . . . . . . (MaxNoBits)supported[4] = 3
. . . . . . . . (MaxSimultaneousTransChsUL)maxSimultaneousTransChs[3] = 2
. . . . . . . . modeSpecificInfo
. . . . . . . . (MaxTransportBlocksUL)maxTransmittedBlocks[4] = 2
. . . . . . . . (MaxNumberOfTFC_UL)maxNumberOfTFC[4] = 3
. . . . . . . . (MaxNumberOfTF)maxNumberOfTF[3] = 0
. . . . . . RF_Capability
. . . . . . . fddRF_Capability
. . . . . . . . (IntegerType)ue_PowerClass[2] = 4
. . . . . . . . (TxRxFrequencySeparation)txRxFrequencySeparation[2] = 0
. . . . . . . tddRF_Capability
. . . . . . PhysicalChannelCapability
. . . . . . . fddPhysChCapability
. . . . . . . . DL_PhysChCapabilityFDD
. . . . . . . . . (IntegerType)maxNoDPCH_PDSCH_Codes[3] = 3
. . . . . . . . . (MaxNoPhysChBitsReceived)maxNoPhysChBitsReceived[4] = 8
. . . . . . . . . (BooleanType)supportForSF_512 = FALSE
. . . . . . . . . (BooleanType)supportOfPDSCH = FALSE
. . . . . . . . . SimultaneousSCCPCH_DPCH_Reception
. . . . . . . . UL_PhysChCapabilityFDD
. . . . . . . . . (MaxNoDPDCH_BitsTransmitted)maxNoDPDCH_BitsTransmitted[4] = 2
. . . . . . . . . (BooleanType)supportOfPCPCH = FALSE
. . . . . . . tddPhysChCapability
. . . . . . UE_MultiModeRAT_Capability
. . . . . . . MultiRAT_Capability
. . . . . . . . (BooleanType)supportOfGSM = FALSE
. . . . . . . . (BooleanType)supportOfMulticarrier = FALSE
. . . . . . . (MultiModeCapability)multiModeCapability[2] = 1
. . . . . . SecurityCapability
. . . . . . . (BitStringType)cipheringAlgorithmCap[16] = '0000000000000011'B
. . . . . . . (BitStringType)integrityProtectionAlgorithmCap[16] = '0000000000000010'B
. . . . . . UE_Positioning_Capability
. . . . . . . (BooleanType)standaloneLocMethodsSupported = FALSE
. . . . . . . (BooleanType)ue_BasedOTDOA_Supported = FALSE
. . . . . . . (NetworkAssistedGPS_Supported)networkAssistedGPS_Supported[2] = 3
. . . . . . . (BooleanType)supportForUE_GPS_TimingOfCellFrames = FALSE
. . . . . . . (BooleanType)supportForIPDL = FALSE
. . . . . . MeasurementCapability
. . . . . . . CompressedModeMeasCapability
. . . . . . . . (BooleanType)fdd_Measurements = FALSE
. . . . . . . . (BooleanType)tdd_Measurements = -
. . . . . . . . GSM_Measurements
. . . . . . . . . (BooleanType)gsm900 = FALSE
. . . . . . . . . (BooleanType)dcs1800 = FALSE
. . . . . . . . . (BooleanType)gsm1900 = FALSE
. . . . . . . . (BooleanType)multiCarrierMeasurements = -
. . . . . . . CompressedModeMeasCapability
. . . . . . . . (BooleanType)fdd_Measurements = FALSE
. . . . . . . . (BooleanType)tdd_Measurements = -
. . . . . . . . GSM_Measurements
. . . . . . . . . (BooleanType)gsm900 = FALSE
. . . . . . . . . (BooleanType)dcs1800 = FALSE
. . . . . . . . . (BooleanType)gsm1900 = FALSE
. . . . . . . . (BooleanType)multiCarrierMeasurements = -
. . . . . v370NonCriticalExtensions
- Constraint:
car_RRC_ConnSetupCmpl
- BinaryMessage:
30 27 02 01 ff 02 01 02 0a 05 01 00 00 00 00 4a 08 00 00 a0 00 05 11 a8 55 06 a4 c2 68 46 2c 94 02 08 00 18 00 11 88 10 00

- No.: 2698
- Timestamp: 12:21:22:088_0
- RFN: 3975
- Chip: 2560
- Event: Cancel Timer
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 10
- Message Structure:
no details available
- Constraint:
t_WaitMS
- BinaryMessage:

- No.: 2699
- Timestamp: 12:21:22:088_1
- RFN: 3975
- Chip: 3072
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ReceiveConnSetupCmpl LINE 10
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2726
- Timestamp: 12:21:22:287_0
- RFN: 3994
- Chip: 36352
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_NAS_UpdateRegistration:lt_MM_Registration LINE 1
- Message Structure:
RRC_DataInd
. (IntegerType)cellId[0] = -1
. (SS_RB_Identity)rB_Id[0] = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain[0] = 0
. (START_Value)start[20] = '00000000000000000000'B
. LOCATIONUPDATINGREQUEST
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)mMProtocolDiscriminator[4] = '0101'B
. . (MsgType)msgType[8] = '00001000'B
. . CiphKeySeqNum
. . . (B1)spare1[1] = '0'B
. . . (KeySeq)keySeq[3] = '000'B
. . LocUpdType
. . . (B1)fOR[1] = '0'B
. . . (B1)spare1[1] = '0'B
. . . (B2)lUT[2] = '00'B
. . LocAreaId_v
. . . (OctetStringType)plmn[3] = '00F110'O
. . . (OctetStringType)lac[2] = '0001'O
. . MS_Clsmk1
. . . (B1)spare1[1] = '0'B
. . . (B2)revLvl[2] = '10'B
. . . (B1)eSIND[1] = '0'B
. . . (B1)a5_1[1] = '1'B
. . . (B3)rFPwrCap[3] = '111'B
. . MS_Identity_lv
. . . (Length)iel[1] = '05'O
. . . (B4)iDigit1[4] = '1111'B
. . . (B1)oddEvenInd[1] = '0'B
. . . (B3)typeOfId[3] = '100'B
. . . (OctetStringType)otherDigits[4] = '12345678'O
. . MS_Clsmk2
. . . (IEI8)iei[8] = '00110011'B
. . . (Length)iel[1] = '03'O
. . . (B1)spare1_1[1] = '0'B
. . . (B2)revLvl[2] = '10'B
. . . (B1)eSIND[1] = '0'B
. . . (B1)a5_1[1] = '1'B
. . . (B3)rFPwrCap[3] = '111'B
. . . (B1)spare1_2[1] = '0'B
. . . (B1)pSCap[1] = '0'B
. . . (B2)sSSI[2] = '01'B
. . . (B1)sMCap[1] = '1'B
. . . (B1)vBS[1] = '0'B
. . . (B1)vGCS[1] = '0'B
. . . (B1)fC[1] = '0'B
. . . (B1)cM3[1] = '1'B
. . . (B1)spare1_3[1] = '0'B
. . . (B1)lCSVA[1] = '0'B
. . . (B1)uCS2[1] = '0'B
. . . (B1)soLSA[1] = '0'B
. . . (B1)cMSP[1] = '0'B
. . . (B1)a5_3[1] = '0'B
. . . (B1)a5_2[1] = '0'B
- Constraint:
car_InitDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 00 03 04 04 00 00 00 05 08 00 00 f1 10 00 01 4f 05 f4 12 34 56 78 33 03 4f 18 80

- No.: 2762
- Timestamp: 12:21:22:293_0
- RFN: 3995
- Chip: 19968
- Event: Send
- PCO: Dc
- Message: RRC_DataReq
- Source: ts_MM_Authentication LINE 2
- Message Structure:
RRC_DataReq
. (IntegerType)cellId[-1] = -1
. (SS_RB_Identity)rB_Id[-1] = 3
. (LogicChGERAN)ch[-1] = -
. (SapId)sapId[1] = -
. (SS_CN_DomainIdentity)cN_Domain[-1] = 0
. AUTHENTICATIONREQUEST
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)mMProtocolDiscriminator[4] = '0101'B
. . (MsgType)msgType[8] = '00010010'B
. . (B4)spare4[4] = '0000'B
. . CiphKeySeqNum
. . . (B1)spare1[1] = '0'B
. . . (KeySeq)keySeq[3] = '001'B
. . (MM_RAND)rAND[128] = '01010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101'B
. . AUTN
. . . (IEI8)iei[8] = '00100000'B
. . . (Length)iel[1] = '10'O
. . . (BitStringType)aUTN[128] = '01010110010100010101000001010011010100100101110100000000000000000101010101010100010101110101011001010001010100000101001101010010'B
- Constraint:
ca_DataReq
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 00 05 12 01 55 55 55 55 55 55 55 55 55 55 55 55 55 55 55 55 20 10 56 51 50 53 52 5d 00 00 55 54 57 56 51 50 53 52

- No.: 2766
- Timestamp: 12:21:23:126_0
- RFN: 4078
- Chip: 34304
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_MM_Authentication LINE 7
- Message Structure:
RRC_DataInd
. (IntegerType)cellId[0] = -1
. (SS_RB_Identity)rB_Id[0] = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain[0] = 0
. (START_Value)start[0] = -
. AUTHENTICATIONRESPONSE
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)mMProtocolDiscriminator[4] = '0101'B
. . (MsgType)msgType[8] = '01010100'B
. . (AuthRsp)authRsp[32] = '01010101010101000101011101010110'B
. . AuthRspExt
- Constraint:
car_UplinkDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 00 05 54 55 54 57 56

- No.: 2808
- Timestamp: 12:21:23:131_3
- RFN: 4079
- Chip: 17408
- Event: Send
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_REQ
- Source: ts_SS_DownloadSecurityKey:lt_DownloadKeyCRLC LINE 1
- Message Structure:
CRLC_SecurityMode_Config_REQ
. (IntegerType)cellId[-1] = -1
. SecurityInfo
. . (CN_DomainIdentity)cn_DomainIdentity[0] = 0
. . (BitStringType)startValue[20] = "00000000000000000000"
. . (BitStringType)cipheringKey[128] = -
. . (BitStringType)integrityKey[128] = '01010111010101100101000101010000010100110101001001011101010111000101111101011110010110010101100001011011010110100101010101010100'B
. . (BitStringType)gsmCipheringKey[64] = -
- Constraint:
ca_CRLC_SecurityModeCfgReq
- BinaryMessage:
30 21 02 01 ff 30 1c 0a 01 00 03 04 04 00 00 00 03 11 00 57 56 51 50 50 52 5d 5c 5c 5e 59 58 58 5a 55 54

- No.: 2809
- Timestamp: 12:21:23:132_0
- RFN: 4079
- Chip: 19200
- Event: Receive
- PCO: CRLC
- Message: CRLC_SecurityMode_Config_CNF
- Source: ts_SS_DownloadSecurityKey:lt_DownloadKeyCRLC LINE 2
- Message Structure:
CRLC_SecurityMode_Config_CNF
. (IntegerType)cellId[0] = -1
- Constraint:
ca_CRLC_SecurityModeCfgCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 2816
- Timestamp: 12:21:23:134_0
- RFN: 4079
- Chip: 27136
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 1
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 0
. (IntegerType)count_I_LSB_UL[-1] = -
. (IntegerType)count_I_LSB_DL[-1] = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 06 02 01 00 02 01 00

- No.: 2817
- Timestamp: 12:21:23:134_1
- RFN: 4079
- Chip: 29184
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 2
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId[0] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 0
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 06 02 01 00

- No.: 2818
- Timestamp: 12:21:23:135_0
- RFN: 4079
- Chip: 30720
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 3
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 1
. (IntegerType)count_I_LSB_UL[-1] = -
. (IntegerType)count_I_LSB_DL[-1] = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 01 02 01 00

- No.: 2819
- Timestamp: 12:21:23:135_1
- RFN: 4079
- Chip: 32000
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 4
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 1
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 2820
- Timestamp: 12:21:23:135_2
- RFN: 4079
- Chip: 33536
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 5
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 2
. (IntegerType)count_I_LSB_UL[-1] = -
. (IntegerType)count_I_LSB_DL[-1] = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 02 02 01 00

- No.: 2821
- Timestamp: 12:21:23:136_0
- RFN: 4079
- Chip: 34816
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 6
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 2822
- Timestamp: 12:21:23:138_0
- RFN: 4080
- Chip: 3072
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 7
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 3
. (IntegerType)count_I_LSB_UL[-1] = -
. (IntegerType)count_I_LSB_DL[-1] = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 03 02 01 00

- No.: 2823
- Timestamp: 12:21:23:138_1
- RFN: 4080
- Chip: 4864
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 8
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 3
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 2824
- Timestamp: 12:21:23:138_2
- RFN: 4080
- Chip: 6400
- Event: Send
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_REQ
- Source: ts_SetDL_RRC_MessageSN LINE 9
- Message Structure:
CRLC_SetRRC_MessageSN_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 4
. (IntegerType)count_I_LSB_UL[-1] = -
. (IntegerType)count_I_LSB_DL[-1] = 0
- Constraint:
ca_DL_CRLC_SetRRC_MSN_REQ
- BinaryMessage:
30 09 02 01 ff 02 01 04 02 01 00

- No.: 2825
- Timestamp: 12:21:23:139_0
- RFN: 4080
- Chip: 7936
- Event: Receive
- PCO: CRLC
- Message: CRLC_SetRRC_MessageSN_CNF
- Source: ts_SetDL_RRC_MessageSN LINE 10
- Message Structure:
CRLC_SetRRC_MessageSN_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 4
- Constraint:
ca_CRLC_SetRRC_MSN_CNF
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 2829
- Timestamp: 12:21:23:141_0
- RFN: 4080
- Chip: 15360
- Event: Send
- PCO: CRLC
- Message: CRLC_Integrity_Activate_REQ
- Source: ts_CRLC_DL_Integrity LINE 1
- Message Structure:
CRLC_Integrity_Activate_REQ
. (IntegerType)cellId[-1] = -1
. (CN_DomainIdentity)cn_DomainIdentity[0] = 0
. IntegrityActivationInfo
. . IntegrityProtectionModeInfo
. . . IntegrityProtectionModeCommand
. . . . startIntegrityProtection
. . . . . (BitStringType)integrityProtInitNumber[32] = "00000000000000000000000000000001"
. . . (IntegrityProtectionAlgorithm)integrityProtectionAlgorithm[0] = 0
- Constraint:
ca_CRLC_DL_IntegrityActivateReq
- BinaryMessage:
30 14 02 01 ff 0a 01 00 30 0c 30 07 03 05 00 00 00 00 01 0a 01 00

- No.: 2830
- Timestamp: 12:21:23:141_1
- RFN: 4080
- Chip: 17152
- Event: Receive
- PCO: CRLC
- Message: CRLC_Integrity_Activate_CNF
- Source: ts_CRLC_DL_Integrity LINE 2
- Message Structure:
CRLC_Integrity_Activate_CNF
. (IntegerType)cellId[0] = -1
- Constraint:
ca_CRLC_IntegrityActivateCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 2837
- Timestamp: 12:21:23:143_0
- RFN: 4080
- Chip: 25344
- Event: Send
- PCO: CRLC
- Message: CRLC_Integrity_Activate_REQ
- Source: ts_RB2_UL_IntegrityActivate LINE 1
- Message Structure:
CRLC_Integrity_Activate_REQ
. (IntegerType)cellId[-1] = -1
. (CN_DomainIdentity)cn_DomainIdentity[0] = 0
. IntegrityActivationInfo
. . IntegrityProtActivationInfoList
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity[-1] = 2
. . . . (IntegerType)rrc_MessageSequenceNumber[-1] = 0
- Constraint:
ca_CRLC_UL_IntegrityActivateReq
- BinaryMessage:
30 10 02 01 ff 0a 01 00 30 08 30 06 02 01 02 02 01 00

- No.: 2838
- Timestamp: 12:21:23:144_0
- RFN: 4080
- Chip: 27136
- Event: Receive
- PCO: CRLC
- Message: CRLC_Integrity_Activate_CNF
- Source: ts_RB2_UL_IntegrityActivate LINE 2
- Message Structure:
CRLC_Integrity_Activate_CNF
. (IntegerType)cellId[0] = -1
- Constraint:
ca_CRLC_IntegrityActivateCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 2845
- Timestamp: 12:21:23:145_1
- RFN: 4080
- Chip: 33024
- Event: Send
- PCO: AM
- Message: RLC_AM_DATA_REQ
- Source: ts_RRC_Security:lt_SendSecurityModeCommand LINE 16
- Message Structure:
RLC_AM_DATA_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 2
. AmConfirmationRequest
. aM_message
. . DL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00000000000000000000000000000000"
. . . . (IntegerType)rrc_MessageSequenceNumber[-1] = 0
. . . DL_DCCH_MessageType
. . . . SecurityModeCommand
. . . . . r3
. . . . . . SecurityModeCommand_r3_IEs
. . . . . . . (IntegerType)rrc_TransactionIdentifier[-1] = 0
. . . . . . . SecurityCapability
. . . . . . . . (BitStringType)cipheringAlgorithmCap[16] = '0000000000000011'B
. . . . . . . . (BitStringType)integrityProtectionAlgorithmCap[16] = '0000000000000010'B
. . . . . . . CipheringModeInfo
. . . . . . . IntegrityProtectionModeInfo
. . . . . . . . IntegrityProtectionModeCommand
. . . . . . . . . startIntegrityProtection
. . . . . . . . . . (BitStringType)integrityProtInitNumber[32] = "00000000000000000000000000000001"
. . . . . . . . (IntegrityProtectionAlgorithm)integrityProtectionAlgorithm[0] = 0
. . . . . . . (CN_DomainIdentity)cn_DomainIdentity[0] = 0
. . . . . . . InterRAT_UE_SecurityCapList
. . . . . . laterNonCriticalExtensions
- Constraint:
cas_RRC_SecModeCmd
- BinaryMessage:
30 17 02 01 ff 02 01 02 05 00 80 00 00 00 04 04 00 01 80 01 40 00 00 00 20

- No.: 2854
- Timestamp: 12:21:23:440_0
- RFN: 4110
- Chip: 11264
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_IND
- Source: ts_RRC_Security:lt_StartSecurity_UE LINE 8
- Message Structure:
RLC_AM_DATA_IND
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
. IntegrityResult
. . (IntegrityStatus)integrityUsed[0] = 0
. aM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "10000001100000001110110111011101"
. . . . (IntegerType)rrc_MessageSequenceNumber[4] = 1
. . . UL_DCCH_MessageType
. . . . SecurityModeComplete
. . . . . (IntegerType)rrc_TransactionIdentifier[2] = 0
. . . . . IntegrityProtActivationInfo
. . . . . . RRC_MessageSequenceNumberList
. . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . (IntegerType)_elem[4] = 0
. . . . . . . (IntegerType)_elem[4] = 0
. . . . . laterNonCriticalExtensions
- Constraint:
car_RRC_SecModeCmpl
- BinaryMessage:
30 12 02 01 ff 02 01 02 0a 01 00 c0 c0 76 ee 8d 21 00 00 00

- No.: 2855
- Timestamp: 12:21:23:440_1
- RFN: 4110
- Chip: 12800
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_Security:lt_StartSecurity_UE LINE 8
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2857
- Timestamp: 12:21:23:441_0
- RFN: 4110
- Chip: 16128
- Event: Send
- PCO: CRLC
- Message: CRLC_Integrity_Activate_REQ
- Source: ts_CRLC_UL_Integrity LINE 1
- Message Structure:
CRLC_Integrity_Activate_REQ
. (IntegerType)cellId[-1] = -1
. (CN_DomainIdentity)cn_DomainIdentity[0] = 0
. IntegrityActivationInfo
. . IntegrityProtActivationInfoList
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity[-1] = 0
. . . . (IntegerType)rrc_MessageSequenceNumber[-1] = 0
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity[-1] = 1
. . . . (IntegerType)rrc_MessageSequenceNumber[-1] = 0
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity[-1] = 3
. . . . (IntegerType)rrc_MessageSequenceNumber[-1] = 0
. . . SS_IntegrityProtActivationTimeInfo
. . . . (IntegerType)rb_Identity[-1] = 4
. . . . (IntegerType)rrc_MessageSequenceNumber[-1] = 0
- Constraint:
ca_CRLC_UL_IntegrityActivateReq
- BinaryMessage:
30 28 02 01 ff 0a 01 00 30 20 30 06 02 01 00 02 01 00 30 06 02 01 01 02 01 00 30 06 02 01 03 02 01 00 30 06 02 01 04 02 01 00

- No.: 2858
- Timestamp: 12:21:23:441_1
- RFN: 4110
- Chip: 17920
- Event: Receive
- PCO: CRLC
- Message: CRLC_Integrity_Activate_CNF
- Source: ts_CRLC_UL_Integrity LINE 2
- Message Structure:
CRLC_Integrity_Activate_CNF
. (IntegerType)cellId[0] = -1
- Constraint:
ca_CRLC_IntegrityActivateCnf
- BinaryMessage:
30 03 02 01 ff

- No.: 2863
- Timestamp: 12:21:23:443_0
- RFN: 4110
- Chip: 22528
- Event: Send
- PCO: Dc
- Message: RRC_DataReq
- Source: ts_NAS_UpdateRegistration:lt_MM_Registration LINE 5
- Message Structure:
RRC_DataReq
. (IntegerType)cellId[-1] = -1
. (SS_RB_Identity)rB_Id[-1] = 3
. (LogicChGERAN)ch[-1] = -
. (SapId)sapId[1] = -
. (SS_CN_DomainIdentity)cN_Domain[-1] = 0
. LOCATIONUPDATINGACCEPT
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)mMProtocolDiscriminator[4] = '0101'B
. . (MsgType)msgType[8] = '00000010'B
. . LocAreaId_v
. . . (OctetStringType)plmn[3] = '00F312'O
. . . (OctetStringType)lac[2] = '0001'O
. . MM_MS_Identity
. . . (IEI8)iei[8] = '00010111'B
. . . (Length)iel[1] = '05'O
. . . (B4)iDigit1[4] = '1111'B
. . . (B1)oddEvenInd[1] = '0'B
. . . (B3)typeOfId[3] = '100'B
. . . (OctetStringType)otherDigits[-1] = '12345678'O
. . (FollowOnProceed)followOnProceed[8] = '10100001'B
. . (CTSPerm)cTSPerm[8] = '10100010'B
. . PLMN_List
- Constraint:
ca_DataReq
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 00 05 02 00 f3 12 00 01 17 05 f4 12 34 56 78 a1 a2

- No.: 2870
- Timestamp: 12:21:23:715_0
- RFN: 4137
- Chip: 29696
- Event: Receive
- PCO: Dc
- Message: RRC_DataInd
- Source: ts_NAS_UpdateRegistration:lt_MM_Registration LINE 6
- Message Structure:
RRC_DataInd
. (IntegerType)cellId[0] = -1
. (SS_RB_Identity)rB_Id[0] = 3
. (LogicChGERAN)ch[0] = -
. (SapId)sapId[0] = -
. (SS_CN_DomainIdentity)cN_Domain[0] = 0
. (START_Value)start[0] = -
. TMSIREALLOCATIONCOMPLETE
. . (SkipIndicator)skipIndicator[4] = '0000'B
. . (ProtocolDiscriminator)mMProtocolDiscriminator[4] = '0101'B
. . (MsgType)msgType[8] = '10011011'B
- Constraint:
car_UplinkDirectTransfer
- BinaryMessage:
ff ff ff ff 00 00 00 03 00 00 00 00 05 9b

- No.: 2881
- Timestamp: 12:21:23:716_4
- RFN: 4137
- Chip: 35584
- Event: Start Timer
- Source: ts_RRC_Delay LINE 1
- Message Structure:
no details available
- Constraint:
t_Dly (1000 Ms)
- BinaryMessage:

- No.: 2885
- Timestamp: 12:21:24:711_0
- RFN: 4237
- Chip: 17920
- Event: Timeout
- Source: ts_RRC_Delay LINE 2
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 2889
- Timestamp: 12:21:24:712_1
- RFN: 4237
- Chip: 22016
- Event: Send
- PCO: UM
- Message: RLC_UM_DATA_REQ
- Source: ts_RRC_ConnRel:lt_Send_RRC_ConnectionRelease LINE 7
- Message Structure:
RLC_UM_DATA_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 1
. uM_message
. . DL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "00000000000000000000000000000000"
. . . . (IntegerType)rrc_MessageSequenceNumber[-1] = 0
. . . DL_DCCH_MessageType
. . . . RRCConnectionRelease
. . . . . r3
. . . . . . RRCConnectionRelease_r3_IEs
. . . . . . . (IntegerType)rrc_TransactionIdentifier[-1] = 0
. . . . . . . (IntegerType)n_308[-1] = -
. . . . . . . (ReleaseCause)releaseCause[0] = 0
. . . . . . . Rplmn_Information
. . . . . . laterNonCriticalExtensions
. (BooleanType)specialLI = FALSE
- Constraint:
cas_RRC_ConnRelDCCH
- BinaryMessage:
30 10 02 01 ff 02 01 01 80 00 00 00 03 c0 00 01 01 00

- No.: 2893
- Timestamp: 12:21:24:887_0
- RFN: 4255
- Chip: 1536
- Event: Receive
- PCO: AM
- Message: RLC_AM_DATA_IND
- Source: ts_RRC_ConnRel:lt_Send_RRC_ConnectionRelease LINE 8
- Message Structure:
RLC_AM_DATA_IND
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
. IntegrityResult
. . (IntegrityStatus)integrityUsed[0] = 0
. aM_message
. . UL_DCCH_Message
. . . IntegrityCheckInfo
. . . . (BitStringType)messageAuthenticationCode[32] = "01000011000100000000100001101011"
. . . . (IntegerType)rrc_MessageSequenceNumber[4] = 2
. . . UL_DCCH_MessageType
. . . . RRCConnectionReleaseComplete
. . . . . (IntegerType)rrc_TransactionIdentifier[2] = 0
. . . . . FailureCauseWithProtErr
. . . . . laterNonCriticalExtensions
- Constraint:
car_RRC_ConnRelCmpl
- BinaryMessage:
30 0f 02 01 ff 02 01 02 0a 01 00 a1 88 04 35 94 40

- No.: 2894
- Timestamp: 12:21:24:888_0
- RFN: 4255
- Chip: 2816
- Event: Log
- PCO: VERDICT
- Message: PREPASS
- Source: ts_RRC_ConnRel:lt_Send_RRC_ConnectionRelease LINE 8
- Message Structure:
no details available
- Constraint:
- BinaryMessage:

- No.: 2897
- Timestamp: 12:21:24:888_3
- RFN: 4255
- Chip: 4608
- Event: Start Timer
- Source: ts_RRC_Delay LINE 1
- Message Structure:
no details available
- Constraint:
t_Dly (1000 Ms)
- BinaryMessage:

- No.: 2901
- Timestamp: 12:21:25:877_0
- RFN: 4354
- Chip: 2048
- Event: Timeout
- Source: ts_RRC_Delay LINE 2
- Message Structure:
no details available
- Constraint:
t_Dly
- BinaryMessage:

- No.: 2908
- Timestamp: 12:21:25:880_0
- RFN: 4354
- Chip: 11776
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 1
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 01 0a 01 00 05 00

- No.: 2912
- Timestamp: 12:21:25:885_0
- RFN: 4354
- Chip: 32256
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 2915
- Timestamp: 12:21:25:886_0
- RFN: 4354
- Chip: 35584
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 2
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 02 0a 01 00 05 00

- No.: 2919
- Timestamp: 12:21:25:895_0
- RFN: 4355
- Chip: 32512
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 2922
- Timestamp: 12:21:25:897_0
- RFN: 4356
- Chip: 2560
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 3
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 03 0a 01 00 05 00

- No.: 2926
- Timestamp: 12:21:25:906_0
- RFN: 4356
- Chip: 35328
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 3
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 2929
- Timestamp: 12:21:25:907_0
- RFN: 4357
- Chip: 512
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 4
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 04 0a 01 00 05 00

- No.: 2933
- Timestamp: 12:21:25:915_0
- RFN: 4357
- Chip: 32000
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 4
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 2936
- Timestamp: 12:21:25:918_0
- RFN: 4358
- Chip: 6400
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 1
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 136
. . . . . UL_RLC_Mode
. . . . . . UL_UM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (NoExplicitDiscard)timerBasedNoExplicit[0] = 9
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 1
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 1
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_UM_Info
- BinaryMessage:
30 22 02 01 ff 02 01 01 0a 01 00 30 17 30 0d 05 00 30 09 02 02 00 88 30 03 0a 01 09 30 06 02 01 01 02 01 01

- No.: 2940
- Timestamp: 12:21:25:925_0
- RFN: 4358
- Chip: 32000
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 2941
- Timestamp: 12:21:25:928_0
- RFN: 4359
- Chip: 6912
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 3
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 2
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 2
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 2
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 02 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 13 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 02 02 01 02

- No.: 2945
- Timestamp: 12:21:25:942_0
- RFN: 4360
- Chip: 22784
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 4
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 2946
- Timestamp: 12:21:25:946_0
- RFN: 4360
- Chip: 37120
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 5
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 3
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 3
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 3
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 03 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 13 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 03 02 01 03

- No.: 2950
- Timestamp: 12:21:25:963_0
- RFN: 4362
- Chip: 26624
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 6
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 3
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 2951
- Timestamp: 12:21:25:967_0
- RFN: 4363
- Chip: 1024
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_SS_RB1_ToRB4_Cfg LINE 7
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 4
. (RatType)ratType[0] = 0
. CrlcConfigReq
. . RBInfo
. . . SS_RLC_Info
. . . . DL_RLC_Mode
. . . . . DL_AM_RLC_Mode
. . . . . . (BooleanType)inSequenceDelivery = TRUE
. . . . . . (ReceivingWindowSize)receivingWindowSize[0] = 3
. . . . . . DL_RLC_StatusInfo
. . . . . . . (TimerStatusProhibit)timerStatusProhibit[0] = 19
. . . . . . . (TimerEPC)timerEPC[0] = -
. . . . . . . (BooleanType)missingPDU_Indicator = TRUE
. . . . . . . (TimerStatusPeriodic)timerStatusPeriodic[0] = -
. . . . SS_DL_RLC_Mode
. . . . . (IntegerType)dl_PayloadSize[-1] = 128
. . . . . UL_RLC_Mode
. . . . . . UL_AM_RLC_Mode
. . . . . . . TransmissionRLC_Discard
. . . . . . . . (MaxDAT)noDiscard[0] = 10
. . . . . . . (TransmissionWindowSize)transmissionWindowSize[0] = 3
. . . . . . . (TimerRST)timerRST[0] = 9
. . . . . . . (MaxRST)max_RST[0] = 0
. . . . . . . PollingInfo
. . . . . . . . (TimerPollProhibit)timerPollProhibit[0] = 19
. . . . . . . . (TimerPoll)timerPoll[0] = 19
. . . . . . . . (Poll_PDU)poll_PDU[0] = -
. . . . . . . . (Poll_SDU)poll_SDU[0] = 0
. . . . . . . . (BooleanType)lastTransmissionPDU_Poll = TRUE
. . . . . . . . (BooleanType)lastRetransmissionPDU_Poll = TRUE
. . . . . . . . (PollWindow)pollWindow[0] = 7
. . . . . . . . (TimerPollPeriodic)timerPollPeriodic[0] = -
. . . RB_LogCH_Mapping
. . . . (IntegerType)uLlogicalChannelIdentity[-1] = 4
. . . . (IntegerType)dLlogicalChannelIdentity[-1] = 4
. . . . (LogicalChannelType)logicalChannelType[0] = -
. . . . (CN_DomainIdentity)cn_DomainIdentity[0] = -
- Constraint:
ca_RB_AM_Info_SRB
- BinaryMessage:
30 4d 02 01 ff 02 01 04 0a 01 00 30 42 30 38 30 0e 01 01 ff 0a 01 03 30 06 0a 01 13 01 01 ff 30 26 02 02 00 80 30 20 0a 01 0a 0a 01 03 0a 01 09 0a 01 00 30 12 0a 01 13 0a 01 13 0a 01 00 01 01 ff 01 01 ff 0a 01 07 30 06 02 01 04 02 01 04

- No.: 2955
- Timestamp: 12:21:25:983_0
- RFN: 4364
- Chip: 25344
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_SS_RB1_ToRB4_Cfg LINE 8
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 4
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 3005
- Timestamp: 12:21:25:991_0
- RFN: 4365
- Chip: 18944
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 0
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 00 02 01 00 0a 01 00 05 00

- No.: 3009
- Timestamp: 12:21:25:994_0
- RFN: 4365
- Chip: 30976
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 0
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 00

- No.: 3012
- Timestamp: 12:21:25:995_2
- RFN: 4365
- Chip: 34560
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_CMAC_Rel LINE 1
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 8
. (RatType)ratType[0] = 0
. configMessage
- Constraint:
cas_MAC_Rel
- BinaryMessage:
30 0b 02 01 00 02 01 08 0a 01 00 05 00

- No.: 3016
- Timestamp: 12:21:26:003_0
- RFN: 4366
- Chip: 27648
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_CMAC_Rel LINE 2
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 8
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 08

- No.: 3019
- Timestamp: 12:21:26:005_0
- RFN: 4366
- Chip: 34560
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Release_REQ
- Source: ts_CPHY_TrChRelNonDch LINE 1
- Message Structure:
CPHY_TrCH_Release_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 8
. TrChConfigType
- Constraint:
ca_PHY_RelReqNonDch
- BinaryMessage:
30 08 02 01 00 02 01 08 05 00

- No.: 3023
- Timestamp: 12:21:26:043_0
- RFN: 4370
- Chip: 23808
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Release_CNF
- Source: ts_CPHY_TrChRelNonDch LINE 2
- Message Structure:
CPHY_TrCH_Release_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 8
- Constraint:
ca_PHY_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 08

- No.: 3026
- Timestamp: 12:21:26:046_0
- RFN: 4370
- Chip: 34304
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 7
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 07

- No.: 3030
- Timestamp: 12:21:26:054_0
- RFN: 4371
- Chip: 25088
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 7
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 07

- No.: 3033
- Timestamp: 12:21:26:056_0
- RFN: 4371
- Chip: 34304
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 8
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 08

- No.: 3037
- Timestamp: 12:21:26:114_0
- RFN: 4377
- Chip: 25600
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 8
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 08

- No.: 3040
- Timestamp: 12:21:26:114_3
- RFN: 4377
- Chip: 28672
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -2
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 00 02 01 fe 0a 01 00 05 00

- No.: 3044
- Timestamp: 12:21:26:117_0
- RFN: 4378
- Chip: 256
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 fe

- No.: 3047
- Timestamp: 12:21:26:118_0
- RFN: 4378
- Chip: 3584
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_CMAC_Rel LINE 1
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 5
. (RatType)ratType[0] = 0
. configMessage
- Constraint:
cas_MAC_Rel
- BinaryMessage:
30 0b 02 01 00 02 01 05 0a 01 00 05 00

- No.: 3051
- Timestamp: 12:21:26:124_0
- RFN: 4378
- Chip: 27136
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_CMAC_Rel LINE 2
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 5
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 05

- No.: 3054
- Timestamp: 12:21:26:127_0
- RFN: 4378
- Chip: 38144
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Release_REQ
- Source: ts_CPHY_TrChRelNonDch LINE 1
- Message Structure:
CPHY_TrCH_Release_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 5
. TrChConfigType
- Constraint:
ca_PHY_RelReqNonDch
- BinaryMessage:
30 08 02 01 00 02 01 05 05 00

- No.: 3058
- Timestamp: 12:21:26:135_0
- RFN: 4379
- Chip: 31744
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Release_CNF
- Source: ts_CPHY_TrChRelNonDch LINE 2
- Message Structure:
CPHY_TrCH_Release_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 5
- Constraint:
ca_PHY_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 05

- No.: 3061
- Timestamp: 12:21:26:136_0
- RFN: 4379
- Chip: 34304
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 6
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 06

- No.: 3065
- Timestamp: 12:21:26:143_0
- RFN: 4380
- Chip: 24832
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 6
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 06

- No.: 3068
- Timestamp: 12:21:26:144_2
- RFN: 4380
- Chip: 27904
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 5
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 05

- No.: 3072
- Timestamp: 12:21:26:153_0
- RFN: 4381
- Chip: 24576
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 5
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 05

- No.: 3077
- Timestamp: 12:21:26:156_0
- RFN: 4381
- Chip: 34048
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 00 02 01 ff 0a 01 00 05 00

- No.: 3081
- Timestamp: 12:21:26:161_0
- RFN: 4382
- Chip: 16640
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 ff

- No.: 3084
- Timestamp: 12:21:26:162_0
- RFN: 4382
- Chip: 20224
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_CMAC_Rel LINE 1
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 4
. (RatType)ratType[0] = 0
. configMessage
- Constraint:
cas_MAC_Rel
- BinaryMessage:
30 0b 02 01 00 02 01 04 0a 01 00 05 00

- No.: 3088
- Timestamp: 12:21:26:165_0
- RFN: 4382
- Chip: 29952
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_CMAC_Rel LINE 2
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 4
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 00 02 01 04

- No.: 3091
- Timestamp: 12:21:26:165_3
- RFN: 4382
- Chip: 32768
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Release_REQ
- Source: ts_CPHY_TrChRelNonDch LINE 1
- Message Structure:
CPHY_TrCH_Release_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 4
. TrChConfigType
- Constraint:
ca_PHY_RelReqNonDch
- BinaryMessage:
30 08 02 01 00 02 01 04 05 00

- No.: 3095
- Timestamp: 12:21:26:172_0
- RFN: 4383
- Chip: 19200
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Release_CNF
- Source: ts_CPHY_TrChRelNonDch LINE 2
- Message Structure:
CPHY_TrCH_Release_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 4
- Constraint:
ca_PHY_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 04

- No.: 3098
- Timestamp: 12:21:26:172_3
- RFN: 4383
- Chip: 21760
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 2
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 02

- No.: 3102
- Timestamp: 12:21:26:176_0
- RFN: 4383
- Chip: 36864
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 2
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 02

- No.: 3105
- Timestamp: 12:21:26:177_2
- RFN: 4384
- Chip: 1024
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 1
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 01

- No.: 3109
- Timestamp: 12:21:26:184_0
- RFN: 4384
- Chip: 26624
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 1
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 01

- No.: 3112
- Timestamp: 12:21:26:184_3
- RFN: 4384
- Chip: 29184
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 4
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 04

- No.: 3116
- Timestamp: 12:21:26:193_0
- RFN: 4385
- Chip: 23552
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 4
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 04

- No.: 3119
- Timestamp: 12:21:26:194_0
- RFN: 4385
- Chip: 26368
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId[-1] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 0
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 00 02 01 00

- No.: 3123
- Timestamp: 12:21:26:197_0
- RFN: 4385
- Chip: 38144
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId[0] = 0
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 0
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 00 02 01 00

- No.: 3177
- Timestamp: 12:21:26:203_2
- RFN: 4386
- Chip: 25600
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 0
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 03 02 01 00 0a 01 00 05 00

- No.: 3181
- Timestamp: 12:21:26:205_0
- RFN: 4386
- Chip: 33792
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 0
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 03 02 01 00

- No.: 3184
- Timestamp: 12:21:26:206_2
- RFN: 4386
- Chip: 36864
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_CMAC_Rel LINE 1
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 8
. (RatType)ratType[0] = 0
. configMessage
- Constraint:
cas_MAC_Rel
- BinaryMessage:
30 0b 02 01 03 02 01 08 0a 01 00 05 00

- No.: 3188
- Timestamp: 12:21:26:210_0
- RFN: 4387
- Chip: 14336
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_CMAC_Rel LINE 2
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId[0] = 3
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 8
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 03 02 01 08

- No.: 3191
- Timestamp: 12:21:26:211_2
- RFN: 4387
- Chip: 16896
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Release_REQ
- Source: ts_CPHY_TrChRelNonDch LINE 1
- Message Structure:
CPHY_TrCH_Release_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 8
. TrChConfigType
- Constraint:
ca_PHY_RelReqNonDch
- BinaryMessage:
30 08 02 01 03 02 01 08 05 00

- No.: 3195
- Timestamp: 12:21:26:242_0
- RFN: 4390
- Chip: 20480
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Release_CNF
- Source: ts_CPHY_TrChRelNonDch LINE 2
- Message Structure:
CPHY_TrCH_Release_CNF
. (IntegerType)cellId[0] = 3
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 8
- Constraint:
ca_PHY_RelCnf
- BinaryMessage:
30 06 02 01 03 02 01 08

- No.: 3198
- Timestamp: 12:21:26:243_0
- RFN: 4390
- Chip: 23808
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 7
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 03 02 01 07

- No.: 3202
- Timestamp: 12:21:26:246_0
- RFN: 4390
- Chip: 35584
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId[0] = 3
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 7
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 03 02 01 07

- No.: 3205
- Timestamp: 12:21:26:246_3
- RFN: 4391
- Chip: 0
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 8
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 03 02 01 08

- No.: 3209
- Timestamp: 12:21:26:302_0
- RFN: 4396
- Chip: 20224
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId[0] = 3
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 8
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 03 02 01 08

- No.: 3212
- Timestamp: 12:21:26:302_3
- RFN: 4396
- Chip: 23296
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -2
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 03 02 01 fe 0a 01 00 05 00

- No.: 3216
- Timestamp: 12:21:26:305_0
- RFN: 4396
- Chip: 32768
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 03 02 01 fe

- No.: 3219
- Timestamp: 12:21:26:306_0
- RFN: 4396
- Chip: 36608
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_CMAC_Rel LINE 1
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 5
. (RatType)ratType[0] = 0
. configMessage
- Constraint:
cas_MAC_Rel
- BinaryMessage:
30 0b 02 01 03 02 01 05 0a 01 00 05 00

- No.: 3223
- Timestamp: 12:21:26:309_0
- RFN: 4397
- Chip: 11776
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_CMAC_Rel LINE 2
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId[0] = 3
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 5
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 03 02 01 05

- No.: 3226
- Timestamp: 12:21:26:310_2
- RFN: 4397
- Chip: 14336
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Release_REQ
- Source: ts_CPHY_TrChRelNonDch LINE 1
- Message Structure:
CPHY_TrCH_Release_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 5
. TrChConfigType
- Constraint:
ca_PHY_RelReqNonDch
- BinaryMessage:
30 08 02 01 03 02 01 05 05 00

- No.: 3230
- Timestamp: 12:21:26:314_0
- RFN: 4397
- Chip: 31232
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Release_CNF
- Source: ts_CPHY_TrChRelNonDch LINE 2
- Message Structure:
CPHY_TrCH_Release_CNF
. (IntegerType)cellId[0] = 3
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 5
- Constraint:
ca_PHY_RelCnf
- BinaryMessage:
30 06 02 01 03 02 01 05

- No.: 3233
- Timestamp: 12:21:26:315_2
- RFN: 4397
- Chip: 34304
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 6
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 03 02 01 06

- No.: 3237
- Timestamp: 12:21:26:319_0
- RFN: 4398
- Chip: 9984
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId[0] = 3
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 6
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 03 02 01 06

- No.: 3240
- Timestamp: 12:21:26:320_0
- RFN: 4398
- Chip: 12544
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 5
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 03 02 01 05

- No.: 3244
- Timestamp: 12:21:26:325_0
- RFN: 4398
- Chip: 32256
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId[0] = 3
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 5
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 03 02 01 05

- No.: 3249
- Timestamp: 12:21:26:326_0
- RFN: 4398
- Chip: 36096
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 03 02 01 ff 0a 01 00 05 00

- No.: 3253
- Timestamp: 12:21:26:329_0
- RFN: 4399
- Chip: 11520
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = 3
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 03 02 01 ff

- No.: 3256
- Timestamp: 12:21:26:330_1
- RFN: 4399
- Chip: 15104
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_CMAC_Rel LINE 1
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 4
. (RatType)ratType[0] = 0
. configMessage
- Constraint:
cas_MAC_Rel
- BinaryMessage:
30 0b 02 01 03 02 01 04 0a 01 00 05 00

- No.: 3260
- Timestamp: 12:21:26:333_0
- RFN: 4399
- Chip: 24576
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_CMAC_Rel LINE 2
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId[0] = 3
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 4
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 03 02 01 04

- No.: 3263
- Timestamp: 12:21:26:333_3
- RFN: 4399
- Chip: 27648
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Release_REQ
- Source: ts_CPHY_TrChRelNonDch LINE 1
- Message Structure:
CPHY_TrCH_Release_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 4
. TrChConfigType
- Constraint:
ca_PHY_RelReqNonDch
- BinaryMessage:
30 08 02 01 03 02 01 04 05 00

- No.: 3267
- Timestamp: 12:21:26:337_0
- RFN: 4400
- Chip: 4352
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Release_CNF
- Source: ts_CPHY_TrChRelNonDch LINE 2
- Message Structure:
CPHY_TrCH_Release_CNF
. (IntegerType)cellId[0] = 3
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 4
- Constraint:
ca_PHY_RelCnf
- BinaryMessage:
30 06 02 01 03 02 01 04

- No.: 3270
- Timestamp: 12:21:26:338_1
- RFN: 4400
- Chip: 6912
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 2
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 03 02 01 02

- No.: 3274
- Timestamp: 12:21:26:342_0
- RFN: 4400
- Chip: 20992
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId[0] = 3
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 2
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 03 02 01 02

- No.: 3277
- Timestamp: 12:21:26:342_3
- RFN: 4400
- Chip: 23808
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 1
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 03 02 01 01

- No.: 3281
- Timestamp: 12:21:26:345_0
- RFN: 4400
- Chip: 35072
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId[0] = 3
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 1
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 03 02 01 01

- No.: 3284
- Timestamp: 12:21:26:346_1
- RFN: 4400
- Chip: 37888
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 4
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 03 02 01 04

- No.: 3288
- Timestamp: 12:21:26:352_0
- RFN: 4401
- Chip: 16896
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId[0] = 3
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 4
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 03 02 01 04

- No.: 3291
- Timestamp: 12:21:26:352_3
- RFN: 4401
- Chip: 19200
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId[-1] = 3
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 0
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 03 02 01 00

- No.: 3295
- Timestamp: 12:21:26:356_0
- RFN: 4401
- Chip: 33024
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId[0] = 3
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 0
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 03 02 01 00

- No.: 3349
- Timestamp: 12:21:26:363_0
- RFN: 4402
- Chip: 21504
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 1
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 01 0a 01 00 05 00

- No.: 3353
- Timestamp: 12:21:26:366_0
- RFN: 4402
- Chip: 32256
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 01

- No.: 3356
- Timestamp: 12:21:26:366_3
- RFN: 4402
- Chip: 35840
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 2
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 02 0a 01 00 05 00

- No.: 3360
- Timestamp: 12:21:26:370_0
- RFN: 4403
- Chip: 9472
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 02

- No.: 3363
- Timestamp: 12:21:26:370_3
- RFN: 4403
- Chip: 12544
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 3
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 03 0a 01 00 05 00

- No.: 3367
- Timestamp: 12:21:26:374_0
- RFN: 4403
- Chip: 27136
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 3
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 03

- No.: 3370
- Timestamp: 12:21:26:375_0
- RFN: 4403
- Chip: 30720
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 4
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 04 0a 01 00 05 00

- No.: 3374
- Timestamp: 12:21:26:378_0
- RFN: 4404
- Chip: 4608
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 4
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 04

- No.: 3378
- Timestamp: 12:21:26:379_2
- RFN: 4404
- Chip: 7936
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 20
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 ff 02 01 14 0a 01 00 05 00

- No.: 3382
- Timestamp: 12:21:26:383_0
- RFN: 4404
- Chip: 22784
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = -1
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 20
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 ff 02 01 14

- No.: 3385
- Timestamp: 12:21:26:384_0
- RFN: 4404
- Chip: 26112
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -3
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 06 02 01 fd 0a 01 00 05 00

- No.: 3389
- Timestamp: 12:21:26:386_0
- RFN: 4404
- Chip: 33536
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -3
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 06 02 01 fd

- No.: 3393
- Timestamp: 12:21:26:387_0
- RFN: 4404
- Chip: 36608
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = 0
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 06 02 01 00 0a 01 00 05 00

- No.: 3397
- Timestamp: 12:21:26:389_0
- RFN: 4405
- Chip: 9216
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[0] = 0
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 06 02 01 00

- No.: 3400
- Timestamp: 12:21:26:390_2
- RFN: 4405
- Chip: 13312
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_CMAC_Rel LINE 1
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 8
. (RatType)ratType[0] = 0
. configMessage
- Constraint:
cas_MAC_Rel
- BinaryMessage:
30 0b 02 01 06 02 01 08 0a 01 00 05 00

- No.: 3404
- Timestamp: 12:21:26:393_0
- RFN: 4405
- Chip: 24064
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_CMAC_Rel LINE 2
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId[0] = 6
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 8
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 06 02 01 08

- No.: 3407
- Timestamp: 12:21:26:394_1
- RFN: 4405
- Chip: 26880
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Release_REQ
- Source: ts_CPHY_TrChRelNonDch LINE 1
- Message Structure:
CPHY_TrCH_Release_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 8
. TrChConfigType
- Constraint:
ca_PHY_RelReqNonDch
- BinaryMessage:
30 08 02 01 06 02 01 08 05 00

- No.: 3411
- Timestamp: 12:21:26:425_0
- RFN: 4408
- Chip: 29952
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Release_CNF
- Source: ts_CPHY_TrChRelNonDch LINE 2
- Message Structure:
CPHY_TrCH_Release_CNF
. (IntegerType)cellId[0] = 6
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 8
- Constraint:
ca_PHY_RelCnf
- BinaryMessage:
30 06 02 01 06 02 01 08

- No.: 3414
- Timestamp: 12:21:26:426_0
- RFN: 4408
- Chip: 33024
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 7
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 06 02 01 07

- No.: 3418
- Timestamp: 12:21:26:429_0
- RFN: 4409
- Chip: 7424
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId[0] = 6
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 7
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 06 02 01 07

- No.: 3421
- Timestamp: 12:21:26:429_3
- RFN: 4409
- Chip: 9984
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 8
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 06 02 01 08

- No.: 3425
- Timestamp: 12:21:26:483_0
- RFN: 4414
- Chip: 25344
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId[0] = 6
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 8
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 06 02 01 08

- No.: 3428
- Timestamp: 12:21:26:484_2
- RFN: 4414
- Chip: 28928
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -2
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 06 02 01 fe 0a 01 00 05 00

- No.: 3432
- Timestamp: 12:21:26:486_0
- RFN: 4414
- Chip: 36352
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -2
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 06 02 01 fe

- No.: 3435
- Timestamp: 12:21:26:487_0
- RFN: 4415
- Chip: 2304
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_CMAC_Rel LINE 1
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 5
. (RatType)ratType[0] = 0
. configMessage
- Constraint:
cas_MAC_Rel
- BinaryMessage:
30 0b 02 01 06 02 01 05 0a 01 00 05 00

- No.: 3439
- Timestamp: 12:21:26:490_0
- RFN: 4415
- Chip: 14336
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_CMAC_Rel LINE 2
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId[0] = 6
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 5
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 06 02 01 05

- No.: 3442
- Timestamp: 12:21:26:491_2
- RFN: 4415
- Chip: 17152
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Release_REQ
- Source: ts_CPHY_TrChRelNonDch LINE 1
- Message Structure:
CPHY_TrCH_Release_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 5
. TrChConfigType
- Constraint:
ca_PHY_RelReqNonDch
- BinaryMessage:
30 08 02 01 06 02 01 05 05 00

- No.: 3446
- Timestamp: 12:21:26:495_0
- RFN: 4415
- Chip: 33792
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Release_CNF
- Source: ts_CPHY_TrChRelNonDch LINE 2
- Message Structure:
CPHY_TrCH_Release_CNF
. (IntegerType)cellId[0] = 6
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 5
- Constraint:
ca_PHY_RelCnf
- BinaryMessage:
30 06 02 01 06 02 01 05

- No.: 3449
- Timestamp: 12:21:26:496_2
- RFN: 4415
- Chip: 36608
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 6
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 06 02 01 06

- No.: 3453
- Timestamp: 12:21:26:501_0
- RFN: 4416
- Chip: 15872
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId[0] = 6
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 6
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 06 02 01 06

- No.: 3456
- Timestamp: 12:21:26:501_3
- RFN: 4416
- Chip: 18432
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 5
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 06 02 01 05

- No.: 3460
- Timestamp: 12:21:26:506_0
- RFN: 4416
- Chip: 36352
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId[0] = 6
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 5
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 06 02 01 05

- No.: 3465
- Timestamp: 12:21:26:507_2
- RFN: 4417
- Chip: 2048
- Event: Send
- PCO: CRLC
- Message: CRLC_Config_REQ
- Source: ts_CRLC_Rel LINE 1
- Message Structure:
CRLC_Config_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[-1] = -1
. (RatType)ratType[0] = 0
. CrlcConfigReq
- Constraint:
ca_CRLC_RB_RelReq
- BinaryMessage:
30 0b 02 01 06 02 01 ff 0a 01 00 05 00

- No.: 3469
- Timestamp: 12:21:26:509_0
- RFN: 4417
- Chip: 9472
- Event: Receive
- PCO: CRLC
- Message: CRLC_Config_CNF
- Source: ts_CRLC_Rel LINE 2
- Message Structure:
CRLC_Config_CNF
. (IntegerType)cellId[0] = 6
. RoutingInfo
. . (IntegerType)rB_Identity[0] = -1
- Constraint:
ca_CRLC_CfgCnf
- BinaryMessage:
30 06 02 01 06 02 01 ff

- No.: 3472
- Timestamp: 12:21:26:510_0
- RFN: 4417
- Chip: 12800
- Event: Send
- PCO: CMAC
- Message: CMAC_Config_REQ
- Source: ts_CMAC_Rel LINE 1
- Message Structure:
CMAC_Config_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 4
. (RatType)ratType[0] = 0
. configMessage
- Constraint:
cas_MAC_Rel
- BinaryMessage:
30 0b 02 01 06 02 01 04 0a 01 00 05 00

- No.: 3476
- Timestamp: 12:21:26:513_0
- RFN: 4417
- Chip: 25344
- Event: Receive
- PCO: CMAC
- Message: CMAC_Config_CNF
- Source: ts_CMAC_Rel LINE 2
- Message Structure:
CMAC_Config_CNF
. (IntegerType)cellId[0] = 6
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 4
- Constraint:
ca_CMAC_CfgCnf
- BinaryMessage:
30 06 02 01 06 02 01 04

- No.: 3479
- Timestamp: 12:21:26:514_0
- RFN: 4417
- Chip: 28416
- Event: Send
- PCO: CPHY
- Message: CPHY_TrCH_Release_REQ
- Source: ts_CPHY_TrChRelNonDch LINE 1
- Message Structure:
CPHY_TrCH_Release_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 4
. TrChConfigType
- Constraint:
ca_PHY_RelReqNonDch
- BinaryMessage:
30 08 02 01 06 02 01 04 05 00

- No.: 3483
- Timestamp: 12:21:26:518_0
- RFN: 4418
- Chip: 3840
- Event: Receive
- PCO: CPHY
- Message: CPHY_TrCH_Release_CNF
- Source: ts_CPHY_TrChRelNonDch LINE 2
- Message Structure:
CPHY_TrCH_Release_CNF
. (IntegerType)cellId[0] = 6
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 4
- Constraint:
ca_PHY_RelCnf
- BinaryMessage:
30 06 02 01 06 02 01 04

- No.: 3486
- Timestamp: 12:21:26:518_3
- RFN: 4418
- Chip: 6656
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 2
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 06 02 01 02

- No.: 3490
- Timestamp: 12:21:26:522_0
- RFN: 4418
- Chip: 21760
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId[0] = 6
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 2
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 06 02 01 02

- No.: 3493
- Timestamp: 12:21:26:523_1
- RFN: 4418
- Chip: 24320
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 1
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 06 02 01 01

- No.: 3497
- Timestamp: 12:21:26:527_0
- RFN: 4419
- Chip: 2048
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId[0] = 6
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 1
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 06 02 01 01

- No.: 3500
- Timestamp: 12:21:26:528_0
- RFN: 4419
- Chip: 5376
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 4
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 06 02 01 04

- No.: 3504
- Timestamp: 12:21:26:532_0
- RFN: 4419
- Chip: 22272
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId[0] = 6
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 4
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 06 02 01 04

- No.: 3507
- Timestamp: 12:21:26:533_2
- RFN: 4419
- Chip: 25088
- Event: Send
- PCO: CPHY
- Message: CPHY_RL_Release_REQ
- Source: ts_SS_StopRL LINE 1
- Message Structure:
CPHY_RL_Release_REQ
. (IntegerType)cellId[-1] = 6
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[-1] = 0
- Constraint:
ca_RL_RelReq
- BinaryMessage:
30 06 02 01 06 02 01 00

- No.: 3511
- Timestamp: 12:21:26:537_0
- RFN: 4420
- Chip: 1280
- Event: Receive
- PCO: CPHY
- Message: CPHY_RL_Release_CNF
- Source: ts_SS_StopRL LINE 2
- Message Structure:
CPHY_RL_Release_CNF
. (IntegerType)cellId[0] = 6
. RoutingInfo
. . (IntegerType)physicalChannelIdentity[0] = 0
- Constraint:
ca_RL_RelCnf
- BinaryMessage:
30 06 02 01 06 02 01 00

- No.: 3536
- Timestamp: 12:21:26:540_2
- RFN: 4420
- Chip: 12288
- Event: Log
- PCO: VERDICT
- Message: PASS
- Source: tc_6_1_1_7 LINE 9
- Message Structure:
no details available
- Constraint:
- BinaryMessage: