| RRC_wk31-tc_6_1_1_7cs_2004-08-17_14.31.44

#### CPHY INI REQ

RRC |  | PHY | @ 00:00:06.030

| Message Details:
RAN Protocol Specification: | 2002-03 R99
| Physical Layer Parameters:
Timing: | Output
Clock: | Output
ISDN Board: | ISDN
| Layer 2 Parameters:
TM bit mode: | enabled

#### MMI_CmdReq

RRC |  | LLA | @ 00:00:06.170

| Message Details:
| MMI_CmdReq:
cmd (IA5String): | Please switch off the UE

#### CPHY INI CNF

PHY |  | RRC | @ 00:00:07.360

| Message Details:
CAPI Version: | 2.10E1_CIPHER
Release: | MX785201A_2_10E1_A_CT_AUG04_A_CIPHER
| MD8480 pool:
| BTS Group 1:
Software: | V5.00h_FH_Cipher
FPGA: | V5.00
| Hardware Slots:
0: | TIMING GENERATOR
1: | TX BASEBAND
2: | TX BASEBAND
3: | TX BASEBAND
4: | FRAME CODER
5: | FRAME CODER
6: | RX BASEBAND
9: | ISDN V5.00
10: | RX BASEBAND
12: | FRAME DECODER
13: | VOICE CODEC
14: | TDMA V5.00b_FH
15: | CPU
| Options:
0: | Tx Diversity
1: | Compressed Mode
2: | Integrity & Ciphering
3: | V5.00
4: | CSD
| Physical Layer Parameters:
Timing: | Output
Clock: | Output
ISDN Board: | ISDN
| BTS Group 2:
Software: | V5.00h_FH_Cipher
FPGA: | V5.00
| Hardware Slots:
0: | TIMING GENERATOR
1: | TX BASEBAND
2: | TX BASEBAND
3: | TX BASEBAND
4: | FRAME CODER
5: | FRAME CODER
6: | RX BASEBAND
9: | ISDN V5.00
10: | RX BASEBAND
12: | FRAME DECODER
13: | VOICE CODEC
14: | TDMA V5.00b_FH
15: | CPU
| Options:
0: | Tx Diversity
1: | Compressed Mode
2: | Integrity & Ciphering
| Physical Layer Parameters:
Timing: | Input
Clock: | Output
ISDN Board: | ISDN

#### MMI_CmdCnf

LLA |  | RRC | @ 00:00:07.560

| Message Details:
| MMI_CmdCnf:
result: | true
resultString (IA5String): | Omit

#### CPHY_Ini_REQ

RRC |  | LLA | @ 00:00:07.560

| Message Details:
CPHY_Ini_REQ: | defaultRadioEnvironment

#### CPHY BTS Configuration REQ

LLA |  | PHY | @ 00:00:07.730

| BTS unit: |  | 1:1
| CFN: |  | 14

| Message Details:
| Configuration Parameters:
Power Mode: | Normal Power Mode
RF Connector: | Main
Baseband Adder: | Off
LVDS: | Off
Timing: | 0
Delta Frequency: | 0
Delta Phase: | 0
| Downlink Parameters:
Frequency: | 2140000000
| Uplink Parameters:
Frequency: | 1950000000
| Tx Parameters:
Baseband Connector: | Analogue
Baseband Delay: | Not Used
| CCH Parameters:
Coder: | Tx Coder1 #1
Baseband: | Tx Baseband1
RF: | Tx RF #1
| DCH Parameters:
Coder: | Tx Coder1 #2
Baseband: | Tx Baseband1
RF: | Tx RF #1
| Rx Parameters:
Baseband Connector: | RF
RxMode: | Simultaneous PRACH/UL_DPCH
| CCH Parameters:
Coder: | Rx Decoder1 #1
Baseband: | Rx Baseband1
RF: | Rx RF #1
| DCH Parameters:
Coder: | Rx Decoder1 #2
Baseband: | Rx Baseband1
RF: | Rx RF #1

#### CPHY BTS Configuration REQ

LLA |  | PHY | @ 00:00:07.700

| BTS unit: |  | 2:2
| CFN: |  | 11

| Message Details:
| Configuration Parameters:
Power Mode: | Normal Power Mode
RF Connector: | Main
Baseband Adder: | On
LVDS: | Off
Timing: | 0
Delta Frequency: | 0
Delta Phase: | 0
| Downlink Parameters:
Frequency: | 0
| Uplink Parameters:
Frequency: | 0
| Tx Parameters:
Baseband Connector: | Analogue
Baseband Delay: | Not Used
| CCH Parameters:
Coder: | Tx Coder2 #1
Baseband: | Tx Baseband2
RF: | Tx RF #2
| DCH Parameters:
Coder: | Tx Coder1 #2
Baseband: | Tx Baseband2
RF: | Tx RF #2
| Rx Parameters:
Baseband Connector: | Not Connected
RxMode: | Simultaneous PRACH/UL_DPCH
| CCH Parameters:
Coder: | Rx Decoder1 #1
Baseband: | Rx Baseband2
RF: | Rx RF #2
| DCH Parameters:
Coder: | Rx Decoder1 #2
Baseband: | Rx Baseband2
RF: | Rx RF #2

#### CPHY BTS Configuration CNF

PHY |  | LLA | @ 00:00:07.730

| BTS unit: |  | 1:1
| CFN: |  | 14

| Message Details:

#### CPHY BTS Configuration REQ

LLA |  | PHY | @ 00:00:07.740

| BTS unit: |  | 1:3
| CFN: |  | 15

| Message Details:
| Configuration Parameters:
Power Mode: | Normal Power Mode
RF Connector: | Main
Baseband Adder: | Off
LVDS: | Off
Timing: | 0
Delta Frequency: | 0
Delta Phase: | 0
| Downlink Parameters:
Frequency: | 2140000000
| Uplink Parameters:
Frequency: | 1950000000
| Tx Parameters:
Baseband Connector: | Not Connected
Baseband Delay: | Not Used
| CCH Parameters:
Coder: | Tx Coder2 #2
Baseband: | Tx Baseband3
RF: | Tx RF #2
| DCH Parameters:
Coder: | Tx Coder1 #2
Baseband: | Tx Baseband3
RF: | Tx RF #2
| Rx Parameters:
Baseband Connector: | Not Connected
RxMode: | Single PRACH/UL_DPCH
| CCH Parameters:
Coder: | Not Used
Baseband: | Not Used
RF: | Not Used
| DCH Parameters:
Coder: | Not Used
Baseband: | Not Used
RF: | Not Used

#### CPHY BTS Configuration REQ

LLA |  | PHY | @ 00:00:07.740

| BTS unit: |  | 1:2
| CFN: |  | 15

| Message Details:
| Configuration Parameters:
Power Mode: | Normal Power Mode
RF Connector: | Main
Baseband Adder: | On
LVDS: | Off
Timing: | 0
Delta Frequency: | 0
Delta Phase: | 0
| Downlink Parameters:
Frequency: | 2140000000
| Uplink Parameters:
Frequency: | 1950000000
| Tx Parameters:
Baseband Connector: | Analogue
Baseband Delay: | Not Used
| CCH Parameters:
Coder: | Tx Coder2 #1
Baseband: | Tx Baseband2
RF: | Tx RF #2
| DCH Parameters:
Coder: | Tx Coder1 #2
Baseband: | Tx Baseband2
RF: | Tx RF #2
| Rx Parameters:
Baseband Connector: | RF
RxMode: | Simultaneous PRACH/UL_DPCH
| CCH Parameters:
Coder: | Rx Decoder1 #1
Baseband: | Rx Baseband2
RF: | Rx RF #2
| DCH Parameters:
Coder: | Rx Decoder1 #2
Baseband: | Rx Baseband2
RF: | Rx RF #2

#### CPHY BTS Configuration CNF

PHY |  | LLA | @ 00:00:07.740

| BTS unit: |  | 1:3
| CFN: |  | 15

| Message Details:

#### CPHY BTS Configuration CNF

PHY |  | LLA | @ 00:00:07.700

| BTS unit: |  | 2:2
| CFN: |  | 11

| Message Details:

#### CPHY BTS Configuration REQ

LLA |  | PHY | @ 00:00:07.710

| BTS unit: |  | 2:1
| CFN: |  | 12

| Message Details:
| Configuration Parameters:
Power Mode: | Normal Power Mode
RF Connector: | Main
Baseband Adder: | Off
LVDS: | Off
Timing: | 0
Delta Frequency: | 0
Delta Phase: | 0
| Downlink Parameters:
Frequency: | 0
| Uplink Parameters:
Frequency: | 0
| Tx Parameters:
Baseband Connector: | Analogue
Baseband Delay: | Not Used
| CCH Parameters:
Coder: | Tx Coder1 #1
Baseband: | Tx Baseband1
RF: | Tx RF #1
| DCH Parameters:
Coder: | Tx Coder1 #2
Baseband: | Tx Baseband1
RF: | Tx RF #1
| Rx Parameters:
Baseband Connector: | RF
RxMode: | Simultaneous PRACH/UL_DPCH
| CCH Parameters:
Coder: | Rx Decoder1 #1
Baseband: | Rx Baseband1
RF: | Rx RF #1
| DCH Parameters:
Coder: | Rx Decoder1 #2
Baseband: | Rx Baseband1
RF: | Rx RF #1

#### CPHY BTS Configuration REQ

LLA |  | PHY | @ 00:00:07.710

| BTS unit: |  | 2:3
| CFN: |  | 12

| Message Details:
| Configuration Parameters:
Power Mode: | Normal Power Mode
RF Connector: | Main
Baseband Adder: | Off
LVDS: | Off
Timing: | 0
Delta Frequency: | 0
Delta Phase: | 0
| Downlink Parameters:
Frequency: | 0
| Uplink Parameters:
Frequency: | 0
| Tx Parameters:
Baseband Connector: | Not Connected
Baseband Delay: | Not Used
| CCH Parameters:
Coder: | Tx Coder2 #2
Baseband: | Tx Baseband3
RF: | Tx RF #2
| DCH Parameters:
Coder: | Tx Coder1 #2
Baseband: | Tx Baseband3
RF: | Tx RF #2
| Rx Parameters:
Baseband Connector: | Not Connected
RxMode: | Single PRACH/UL_DPCH
| CCH Parameters:
Coder: | Not Used
Baseband: | Not Used
RF: | Not Used
| DCH Parameters:
Coder: | Not Used
Baseband: | Not Used
RF: | Not Used

#### CPHY BTS Configuration CNF

PHY |  | LLA | @ 00:00:07.710

| BTS unit: |  | 2:1
| CFN: |  | 12

| Message Details:

#### CPHY BTS Attenuation REQ

LLA |  | PHY | @ 00:00:07.750

| BTS unit: |  | 1:1
| CFN: |  | 16

| Message Details:
| Configuration Parameters:
Tx Attenuation In dB: | 2
Rx Reference Power In dBm: | 0

#### CPHY BTS Configuration CNF

PHY |  | LLA | @ 00:00:07.750

| BTS unit: |  | 1:2
| CFN: |  | 16

| Message Details:

#### CPHY BTS Attenuation CNF

PHY |  | LLA | @ 00:00:07.760

| BTS unit: |  | 1:1
| CFN: |  | 17

| Message Details:

#### CPHY BTS Configuration CNF

PHY |  | LLA | @ 00:00:07.720

| BTS unit: |  | 2:3
| CFN: |  | 13

| Message Details:

#### CPHY BTS Attenuation REQ

LLA |  | PHY | @ 00:00:07.750

| BTS unit: |  | 2:2
| CFN: |  | 16

| Message Details:
| Configuration Parameters:
Tx Attenuation In dB: | 2
Rx Reference Power In dBm: | 0

#### CPHY BTS Attenuation CNF

PHY |  | LLA | @ 00:00:07.750

| BTS unit: |  | 2:2
| CFN: |  | 16

| Message Details:

#### CPHY BTS Attenuation REQ

LLA |  | PHY | @ 00:00:07.760

| BTS unit: |  | 2:1
| CFN: |  | 17

| Message Details:
| Configuration Parameters:
Tx Attenuation In dB: | 2
Rx Reference Power In dBm: | 0

#### CPHY BTS Attenuation CNF

PHY |  | LLA | @ 00:00:07.760

| BTS unit: |  | 2:1
| CFN: |  | 17

| Message Details:

#### CPHY BTS Attenuation REQ

LLA |  | PHY | @ 00:00:07.830

| BTS unit: |  | 1:2
| CFN: |  | 24

| Message Details:
| Configuration Parameters:
Tx Attenuation In dB: | 2
Rx Reference Power In dBm: | 0

#### CPHY BTS Attenuation CNF

PHY |  | LLA | @ 00:00:07.830

| BTS unit: |  | 1:2
| CFN: |  | 24

| Message Details:

#### CPHY_Ini_CNF

LLA |  | RRC | @ 00:00:07.980

| Message Details:
| CPHY_Ini_CNF:
confirmation: |

#### CPHY_Cell_Config_REQ

RRC |  | LLA | @ 00:00:07.980

| Cell ID: |  | 0

| Message Details:
| CPHY_Cell_Config_REQ:
cellId: | 0
tcell: | 0
sfnOffset: | 0
| frequencyInfo:
| modeSpecificInfo:
| fdd: (FrequencyInfoFDD)
uarfcn_UL (UARFCN): | 9613
uarfcn_DL (UARFCN): | 10563
primaryScramblingCode_SS: | 100
| cellTxPowerLevel:
defaultCellTxPowerLvl: |
dLTxAttenuationLevel: | 8

#### CPHY BTS Frequency REQ

LLA |  | PHY | @ 00:00:07.990

| BTS unit: |  | 1:1
| CFN: |  | 40

| Message Details:
| Configuration Parameters:
Down Link Frequency: | 2112600000
Up Link Frequency: | 1922600000

#### CPHY BTS Frequency CNF

PHY |  | LLA | @ 00:00:07.990

| BTS unit: |  | 1:1
| CFN: |  | 40

| Message Details:

#### CPHY_Cell_Config_CNF

LLA |  | RRC | @ 00:00:08.000

| Cell ID: |  | 0

| Message Details:
| CPHY_Cell_Config_CNF:
cellId: | 0

#### CPHY_RL_Setup_REQ

RRC |  | LLA | @ 00:00:08.000

| Channel ID: |  | P-CPICH
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_REQ:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 0
ratType: | fdd
| setupMessage: (CphyRlSetupReq)
| physicalChannelInfo:
| primaryCPICHInfo:
dl_TxPower_PCPICH: | -60
txdiversityIndicator: | false

#### CPHY Radio Link Setup REQ

LLA |  | PHY | @ 00:00:08.010

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: P_CPICH
| CFN: |  | 42

| Message Details:
| Configuration Parameters:
Channel Offset: | 7680
Scrambling Code: | 1600
Symbol Rate: | 15k
Channelization Code: | 0
Adjust Time: | 0
Power in dBm: | -48
Tx Diversity: | Off
NumOfDpdch: | 0

#### CPHY Radio Link Setup CNF

PHY |  | LLA | @ 00:00:08.010

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: P_CPICH
| CFN: |  | 42

| Message Details:

#### CPHY_RL_Setup_CNF

LLA |  | RRC | @ 00:00:08.030

| Channel ID: |  | P-CPICH
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_CNF:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 0

#### CPHY_RL_Setup_REQ

RRC |  | LLA | @ 00:00:08.030

| Channel ID: |  | P-SCH
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_REQ:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 1
ratType: | fdd
| setupMessage: (CphyRlSetupReq)
| physicalChannelInfo:
| primarySCHInfo:
tstdIndicator: | false
dl_TxPower: | -5

#### CPHY_RL_Setup_CNF

LLA |  | RRC | @ 00:00:08.040

| Channel ID: |  | P-SCH
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_CNF:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 1

#### CPHY_RL_Setup_REQ

RRC |  | LLA | @ 00:00:08.040

| Channel ID: |  | S-SCH
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_REQ:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 2
ratType: | fdd
| setupMessage: (CphyRlSetupReq)
| physicalChannelInfo:
| secondarySCHInfo:
tstdIndicator: | false
dl_TxPower: | -5

#### CPHY Radio Link Setup REQ

LLA |  | PHY | @ 00:00:08.040

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: P_SCH
| CFN: |  | 45

| Message Details:
| Configuration Parameters:
Channel Offset: | 7680
Adjust Time: | 0
Power in dBm: | -53
Tx Diversity: | Off
NumOfDpdch: | 0

#### CPHY Radio Link Setup CNF

PHY |  | LLA | @ 00:00:08.040

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: P_SCH
| CFN: |  | 45

| Message Details:

#### CPHY Radio Link Setup REQ

LLA |  | PHY | @ 00:00:08.050

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: S_SCH
| CFN: |  | 46

| Message Details:
| Configuration Parameters:
Channel Offset: | 7680
Adjust Time: | 0
Power in dBm: | -53
Tx Diversity: | Off
NumOfDpdch: | 0

#### CPHY Radio Link Setup CNF

PHY |  | LLA | @ 00:00:08.050

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: S_SCH
| CFN: |  | 46

| Message Details:

#### CPHY_RL_Setup_CNF

LLA |  | RRC | @ 00:00:08.060

| Channel ID: |  | S-SCH
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_CNF:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 2

#### CPHY_RL_Setup_REQ

RRC |  | LLA | @ 00:00:08.060

| Channel ID: |  | P-CCPCH
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_REQ:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 4
ratType: | fdd
| setupMessage: (CphyRlSetupReq)
| physicalChannelInfo:
| primaryCCPCHInfo:
sttd_Indicator: | false
dl_TxPower: | -2

#### CPHY Radio Link Setup REQ

LLA |  | PHY | @ 00:00:08.070

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: P_CCPCH
| CFN: |  | 48

| Message Details:
| Configuration Parameters:
Channel Offset: | 7680
SFN Offset: | 0
Scrambling Code: | 1600
Symbol Rate: | 15k
Channelization Code: | 1
Adjust Time: | 0
Power in dBm: | -50
Tx Diversity: | Off
NumOfDpdch: | 1

#### CPHY Radio Link Setup CNF

PHY |  | LLA | @ 00:00:08.070

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: P_CCPCH
| CFN: |  | 48

| Message Details:

#### CPHY_RL_Setup_CNF

LLA |  | RRC | @ 00:00:08.080

| Channel ID: |  | P-CCPCH
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_CNF:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 4

#### CPHY_TrCH_Config_REQ

RRC |  | LLA | @ 00:00:08.080

| Channel ID: |  | P-CCPCH
| Cell ID: |  | 0

| Message Details:
| CPHY_TrCH_Config_REQ:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 4
ratType: | fdd
| trchConfigType:
nonDch: |
| configMessage: (CphyTrchConfigReq)
| activationTime: (SS_ActivationTime)
activateNow: |
| ulconnectedTrCHList: Omit
| ulTFCS: (TFCS) Omit
| dlconnectedTrCHList:
| :
trchid (TransportChannelIdentity): | 11
dl_TransportChannelType (SS_DL_TransportChannelType): | bch
| transportChannelInfo: (CommonOrDedicatedTFS)
| tti:
| tti20: (CommonOrDedicatedTF_InfoList)
| CommonOrDedicatedTF_Info:
tb_Size: | 246
| numberOfTbSizeList:
| NumberOfTransportBlocks:
one: |
| logicalChannelList:
configured: |
| semistaticTF_Information:
| channelCodingType:
convolutional (CodingRate): | half
rateMatchingAttribute: | 1
crc_Size: | crc16
| dlTFCS: (TFCS)
| normalTFCI_Signalling: (ExplicitTFCS_Configuration)
| complete: (TFCS_ReconfAdd)
| ctfcSize:
| ctfc2Bit:
| :
ctfc2: | 0
| powerOffsetInformation:
| gainFactorInformation:
| signalledGainFactors:
| modeSpecificInfo:
| fdd:
gainFactorBetaC (GainFactor): | 11
gainFactorBetaD (GainFactor): | 15
referenceTFC_ID: | 0
powerOffsetPp_m: | Omit

#### CPHY Transport Channel Configuration REQ

LLA |  | PHY | @ 00:00:08.090

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: P_CCPCH
| CFN: |  | 50

| Message Details:
| Configuration Parameters:
DTX Position: | Flexible
Second Interleave: | On
Puncture Limit: | 0
CCTrCH Length: | 270
Number Of Transport Channels: | 1
| Transport Channels:
| Item Number 0:
| Transport Channel Parameters:
| Transport Channel:
Name: | BCH
Identity: | 0
TTI (ms): | 20
EP Type: | 1/2 Rate Convolutional Coding
CRC Size: | 16
RM Attribute: | 1
First Interleave: | On
Number Of Transport Formats: | 2
| Transport Format Set:
| Transport Format 0:
Number Of Transport Blocks: | 0
Transport Block Size In Bits: | 0
| Transport Format 1:
Number Of Transport Blocks: | 1
Transport Block Size In Bits: | 246
RM Maximum Length: | 540
| Transport Format Combination Set:
Number Of Transport Format Combinations: | 2
| Transport Format Combinations 0:
Transport Format: | 0
| Transport Format Combinations 1:
Transport Format: | 1

#### CPHY Transport Channel Configuration CNF

PHY |  | LLA | @ 00:00:08.090

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: P_CCPCH
| CFN: |  | 50

| Message Details:

#### CPHY_TrCH_Config_CNF

LLA |  | RRC | @ 00:00:08.110

| Channel ID: |  | P-CCPCH
| Cell ID: |  | 0

| Message Details:
| CPHY_TrCH_Config_CNF:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 4

#### CMAC_Config_REQ

RRC |  | LLA | @ 00:00:08.110

| Channel ID: |  | P-CCPCH
| Cell ID: |  | 0

| Message Details:
| CMAC_Config_REQ:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 4
ratType: | fdd
| configMessage:
| setup: (CmacConfigReq)
| activationTime: (SS_ActivationTime)
activateNow: |
| uE_Info:
| u_RNTI: Omit
c_RNTI: | Omit
| trCHInfo:
| ulconnectedTrCHList: Omit
| ulTFCS: (TFCS) Omit
| dlconnectedTrCHList:
| :
trchid (TransportChannelIdentity): | 11
| transportChannelInfo: (CommonOrDedicatedTFS)
| tti:
| tti20: (CommonOrDedicatedTF_InfoList)
| CommonOrDedicatedTF_Info:
tb_Size: | 246
| numberOfTbSizeList:
| NumberOfTransportBlocks:
one: |
| logicalChannelList:
configured: |
| semistaticTF_Information:
| channelCodingType:
convolutional (CodingRate): | half
rateMatchingAttribute: | 1
crc_Size: | crc16
| dlTFCS: (TFCS)
| normalTFCI_Signalling: (ExplicitTFCS_Configuration)
| complete: (TFCS_ReconfAdd)
| ctfcSize:
| ctfc2Bit:
| :
ctfc2: | 0
| powerOffsetInformation:
| gainFactorInformation:
| signalledGainFactors:
| modeSpecificInfo:
| fdd:
gainFactorBetaC (GainFactor): | 11
gainFactorBetaD (GainFactor): | 15
referenceTFC_ID: | 0
powerOffsetPp_m: | Omit
| trCH_LogCHMapping: (TrCH_LogCHMappingList1)
| ulconnectedTrCHList: Omit
| dlconnectedTrCHList:
| :
trchid (TransportChannelIdentity): | 11
| trCH_LogCHMappingList:
| TrCH_LogicalChannelMapping:
| logicalChannel_Mapping:
| dl_LogicalChannelMapping: (SS_DL_LogicalChannelMapping)
macHeaderManipulation (MAC_HeaderManipulation): | normalMacHeader
dl_TransportChannelType (SS_DL_TransportChannelType): | bch
logicalChannelIdentity: | 1
logicalChannelType: | bCCH
| rlc_SizeList:
configured: |
mac_LogicalChannelPriority: | 1
rB_Identity: | -1
cn_DomainIdentity: | Omit

#### CMAC Configuration REQ

LLA |  | MAC | @ 00:00:08.120

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: P_CCPCH
| CFN: |  | 53

| Message Details:
| Configuration Parameters:
Number Of Transport Channels: | 1
| Transport Channels:
| Item Number 0:
| Transport Channel Parameters:
| Transport Channel:
Name: | BCH
Identity: | 0
TTI (ms): | 20
EP Type: | 1/2 Rate Convolutional Coding
CRC Size: | 16
RM Attribute: | 1
First Interleave: | On
Number Of Transport Formats: | 2
| Transport Format Set:
| Transport Format 0:
Number Of Transport Blocks: | 0
Transport Block Size In Bits: | 0
| Transport Format 1:
Number Of Transport Blocks: | 1
Transport Block Size In Bits: | 246
Number Of Logical Channels: | 1
| Logical Channels:
| Item Number 0:
| Logical Channel:
Name: | BCCH
Identity: | 0
Priority: | 1
CT Length: | 0
CT Value: | 0
TCTF Length: | 0
TCTF Value: | 0
UE ID Type: | Not used
UE ID: | 0
Active Flag: | 1
| Transport Format Combination Set:
Number Of Transport Format Combinations: | 2
| Transport Format Combinations 0:
Transport Format: | 0
| Transport Format Combinations 1:
Transport Format: | 1

#### CMAC Configuration CNF

MAC |  | LLA | @ 00:00:08.120

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: P_CCPCH
| CFN: |  | 53

| Message Details:

#### CMAC_Config_CNF

LLA |  | RRC | @ 00:00:08.140

| Channel ID: |  | P-CCPCH
| Cell ID: |  | 0

| Message Details:
| CMAC_Config_CNF:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 4

#### CPHY_RL_Setup_REQ

RRC |  | LLA | @ 00:00:08.140

| Channel ID: |  | S-CCPCH#1
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_REQ:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 5
ratType: | fdd
| setupMessage: (CphyRlSetupReq)
| physicalChannelInfo:
| secondaryCCPCHInfo:
scramblingCode: | 0
| dl_ChannelizationCode: (SF256_AndCodeNumber)
sf64: | 1
sCCPCHSlotFormat: | 8
timingOffset: | 0
positionFixedOrFlexible: | flexible
sttd_Indicator: | false
dl_TxPower: | -2
powerOffsetOfTFCI_PO1: | 6
powerOffsetOfPILOT_PO3: | 6

#### CPHY_RL_Setup_CNF

LLA |  | RRC | @ 00:00:08.150

| Channel ID: |  | S-CCPCH#1
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_CNF:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 5

#### CPHY_TrCH_Config_REQ

RRC |  | LLA | @ 00:00:08.150

| Channel ID: |  | S-CCPCH#1
| Cell ID: |  | 0

| Message Details:
| CPHY_TrCH_Config_REQ:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 5
ratType: | fdd
| trchConfigType:
nonDch: |
| configMessage: (CphyTrchConfigReq)
| activationTime: (SS_ActivationTime)
activateNow: |
| ulconnectedTrCHList: Omit
| ulTFCS: (TFCS) Omit
| dlconnectedTrCHList:
| :
trchid (TransportChannelIdentity): | 12
dl_TransportChannelType (SS_DL_TransportChannelType): | pch
| transportChannelInfo: (CommonOrDedicatedTFS)
| tti:
| tti10: (CommonOrDedicatedTF_InfoList)
| CommonOrDedicatedTF_Info:
tb_Size: | 240
| numberOfTbSizeList:
| NumberOfTransportBlocks:
zero: |
| NumberOfTransportBlocks:
one: |
| logicalChannelList:
allSizes: |
| semistaticTF_Information:
| channelCodingType:
convolutional (CodingRate): | half
rateMatchingAttribute: | 230
crc_Size: | crc16
| :
trchid (TransportChannelIdentity): | 13
dl_TransportChannelType (SS_DL_TransportChannelType): | fach
| transportChannelInfo: (CommonOrDedicatedTFS)
| tti:
| tti10: (CommonOrDedicatedTF_InfoList)
| CommonOrDedicatedTF_Info:
tb_Size: | 168
| numberOfTbSizeList:
| NumberOfTransportBlocks:
zero: |
| NumberOfTransportBlocks:
one: |
| NumberOfTransportBlocks:
small: | 2
| logicalChannelList:
allSizes: |
| semistaticTF_Information:
| channelCodingType:
convolutional (CodingRate): | half
rateMatchingAttribute: | 220
crc_Size: | crc16
| :
trchid (TransportChannelIdentity): | 14
dl_TransportChannelType (SS_DL_TransportChannelType): | fach
| transportChannelInfo: (CommonOrDedicatedTFS)
| tti:
| tti10: (CommonOrDedicatedTF_InfoList)
| CommonOrDedicatedTF_Info:
tb_Size: | 360
| numberOfTbSizeList:
| NumberOfTransportBlocks:
zero: |
| NumberOfTransportBlocks:
one: |
| logicalChannelList:
allSizes: |
| semistaticTF_Information:
| channelCodingType:
turbo: |
rateMatchingAttribute: | 130
crc_Size: | crc16
| dlTFCS: (TFCS)
| normalTFCI_Signalling: (ExplicitTFCS_Configuration)
| complete: (TFCS_ReconfAdd)
| ctfcSize:
| ctfc4Bit:
| :
ctfc4: | 0
| powerOffsetInformation:
| gainFactorInformation:
computedGainFactors (ReferenceTFC_ID): | 0
powerOffsetPp_m: | Omit
| :
ctfc4: | 1
| powerOffsetInformation:
| gainFactorInformation:
computedGainFactors (ReferenceTFC_ID): | 0
powerOffsetPp_m: | Omit
| :
ctfc4: | 2
| powerOffsetInformation:
| gainFactorInformation:
computedGainFactors (ReferenceTFC_ID): | 0
powerOffsetPp_m: | Omit
| :
ctfc4: | 3
| powerOffsetInformation:
| gainFactorInformation:
computedGainFactors (ReferenceTFC_ID): | 0
powerOffsetPp_m: | Omit
| :
ctfc4: | 4
| powerOffsetInformation:
| gainFactorInformation:
computedGainFactors (ReferenceTFC_ID): | 0
powerOffsetPp_m: | Omit
| :
ctfc4: | 5
| powerOffsetInformation:
| gainFactorInformation:
computedGainFactors (ReferenceTFC_ID): | 0
powerOffsetPp_m: | Omit
| :
ctfc4: | 6
| powerOffsetInformation:
| gainFactorInformation:
computedGainFactors (ReferenceTFC_ID): | 0
powerOffsetPp_m: | Omit
| :
ctfc4: | 8
| powerOffsetInformation:
| gainFactorInformation:
| signalledGainFactors:
| modeSpecificInfo:
| fdd:
gainFactorBetaC (GainFactor): | 11
gainFactorBetaD (GainFactor): | 15
referenceTFC_ID: | 0
powerOffsetPp_m: | Omit

#### CPHY Radio Link Setup REQ

LLA |  | PHY | @ 00:00:08.150

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: S_CCPCH
| CFN: |  | 56

| Message Details:
| Configuration Parameters:
Channel Offset: | 7680
Scrambling Code: | 1600
Symbol Rate: | 60k
Channelization Code: | 1
Adjust Time: | 0
Power in dBm: | -50
Tx Diversity: | Off
Slot Format: | 8
NumOfDpdch: | 1

#### CPHY Radio Link Setup CNF

PHY |  | LLA | @ 00:00:08.150

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: S_CCPCH
| CFN: |  | 56

| Message Details:

#### CPHY Transport Channel Configuration REQ

LLA |  | PHY | @ 00:00:08.170

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: S_CCPCH
| CFN: |  | 58

| Message Details:
| Configuration Parameters:
DTX Position: | Flexible
Second Interleave: | On
Puncture Limit: | 100
CCTrCH Length: | 1080
Number Of Transport Channels: | 3
| Transport Channels:
| Item Number 0:
| Transport Channel Parameters:
| Transport Channel:
Name: | PCH
Identity: | 0
TTI (ms): | 10
EP Type: | 1/2 Rate Convolutional Coding
CRC Size: | 16
RM Attribute: | 230
First Interleave: | On
Number Of Transport Formats: | 2
| Transport Format Set:
| Transport Format 0:
Number Of Transport Blocks: | 0
Transport Block Size In Bits: | 240
| Transport Format 1:
Number Of Transport Blocks: | 1
Transport Block Size In Bits: | 240
RM Maximum Length: | 457
| Item Number 1:
| Transport Channel Parameters:
| Transport Channel:
Name: | FACH
Identity: | 0
TTI (ms): | 10
EP Type: | 1/2 Rate Convolutional Coding
CRC Size: | 16
RM Attribute: | 220
First Interleave: | On
Number Of Transport Formats: | 3
| Transport Format Set:
| Transport Format 0:
Number Of Transport Blocks: | 0
Transport Block Size In Bits: | 168
| Transport Format 1:
Number Of Transport Blocks: | 1
Transport Block Size In Bits: | 168
| Transport Format 2:
Number Of Transport Blocks: | 2
Transport Block Size In Bits: | 168
RM Maximum Length: | 623
| Item Number 2:
| Transport Channel Parameters:
| Transport Channel:
Name: | FACH
Identity: | 1
TTI (ms): | 10
EP Type: | Turbo Coding
CRC Size: | 16
RM Attribute: | 130
First Interleave: | On
Number Of Transport Formats: | 2
| Transport Format Set:
| Transport Format 0:
Number Of Transport Blocks: | 0
Transport Block Size In Bits: | 360
| Transport Format 1:
Number Of Transport Blocks: | 1
Transport Block Size In Bits: | 360
RM Maximum Length: | 558
| Transport Format Combination Set:
Number Of Transport Format Combinations: | 8
| Transport Format Combinations 0:
Transport Format: | 0
Transport Format: | 0
Transport Format: | 0
| Transport Format Combinations 1:
Transport Format: | 1
Transport Format: | 0
Transport Format: | 0
| Transport Format Combinations 2:
Transport Format: | 0
Transport Format: | 1
Transport Format: | 0
| Transport Format Combinations 3:
Transport Format: | 1
Transport Format: | 1
Transport Format: | 0
| Transport Format Combinations 4:
Transport Format: | 0
Transport Format: | 2
Transport Format: | 0
| Transport Format Combinations 5:
Transport Format: | 1
Transport Format: | 2
Transport Format: | 0
| Transport Format Combinations 6:
Transport Format: | 0
Transport Format: | 0
Transport Format: | 1
| Transport Format Combinations 7:
Transport Format: | 0
Transport Format: | 1
Transport Format: | 1

#### CPHY Transport Channel Configuration CNF

PHY |  | LLA | @ 00:00:08.170

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: S_CCPCH
| CFN: |  | 58

| Message Details:

#### CPHY_TrCH_Config_CNF

LLA |  | RRC | @ 00:00:08.190

| Channel ID: |  | S-CCPCH#1
| Cell ID: |  | 0

| Message Details:
| CPHY_TrCH_Config_CNF:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 5

#### CMAC_Config_REQ

RRC |  | LLA | @ 00:00:08.190

| Channel ID: |  | S-CCPCH#1
| Cell ID: |  | 0

| Message Details:
| CMAC_Config_REQ:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 5
ratType: | fdd
| configMessage:
| setup: (CmacConfigReq)
| activationTime: (SS_ActivationTime)
activateNow: |
| uE_Info:
| u_RNTI:
srnc_Identity: | 000000000001
s_RNTI: | 00000000000000000001
c_RNTI: | 0000000000000001
| trCHInfo:
| ulconnectedTrCHList: Omit
| ulTFCS: (TFCS) Omit
| dlconnectedTrCHList:
| :
trchid (TransportChannelIdentity): | 12
| transportChannelInfo: (CommonOrDedicatedTFS)
| tti:
| tti10: (CommonOrDedicatedTF_InfoList)
| CommonOrDedicatedTF_Info:
tb_Size: | 240
| numberOfTbSizeList:
| NumberOfTransportBlocks:
zero: |
| NumberOfTransportBlocks:
one: |
| logicalChannelList:
allSizes: |
| semistaticTF_Information:
| channelCodingType:
convolutional (CodingRate): | half
rateMatchingAttribute: | 230
crc_Size: | crc16
| :
trchid (TransportChannelIdentity): | 13
| transportChannelInfo: (CommonOrDedicatedTFS)
| tti:
| tti10: (CommonOrDedicatedTF_InfoList)
| CommonOrDedicatedTF_Info:
tb_Size: | 168
| numberOfTbSizeList:
| NumberOfTransportBlocks:
zero: |
| NumberOfTransportBlocks:
one: |
| NumberOfTransportBlocks:
small: | 2
| logicalChannelList:
allSizes: |
| semistaticTF_Information:
| channelCodingType:
convolutional (CodingRate): | half
rateMatchingAttribute: | 220
crc_Size: | crc16
| :
trchid (TransportChannelIdentity): | 14
| transportChannelInfo: (CommonOrDedicatedTFS)
| tti:
| tti10: (CommonOrDedicatedTF_InfoList)
| CommonOrDedicatedTF_Info:
tb_Size: | 360
| numberOfTbSizeList:
| NumberOfTransportBlocks:
zero: |
| NumberOfTransportBlocks:
one: |
| logicalChannelList:
allSizes: |
| semistaticTF_Information:
| channelCodingType:
turbo: |
rateMatchingAttribute: | 130
crc_Size: | crc16
| dlTFCS: (TFCS)
| normalTFCI_Signalling: (ExplicitTFCS_Configuration)
| complete: (TFCS_ReconfAdd)
| ctfcSize:
| ctfc4Bit:
| :
ctfc4: | 0
| powerOffsetInformation:
| gainFactorInformation:
computedGainFactors (ReferenceTFC_ID): | 0
powerOffsetPp_m: | Omit
| :
ctfc4: | 1
| powerOffsetInformation:
| gainFactorInformation:
computedGainFactors (ReferenceTFC_ID): | 0
powerOffsetPp_m: | Omit
| :
ctfc4: | 2
| powerOffsetInformation:
| gainFactorInformation:
computedGainFactors (ReferenceTFC_ID): | 0
powerOffsetPp_m: | Omit
| :
ctfc4: | 3
| powerOffsetInformation:
| gainFactorInformation:
computedGainFactors (ReferenceTFC_ID): | 0
powerOffsetPp_m: | Omit
| :
ctfc4: | 4
| powerOffsetInformation:
| gainFactorInformation:
computedGainFactors (ReferenceTFC_ID): | 0
powerOffsetPp_m: | Omit
| :
ctfc4: | 5
| powerOffsetInformation:
| gainFactorInformation:
computedGainFactors (ReferenceTFC_ID): | 0
powerOffsetPp_m: | Omit
| :
ctfc4: | 6
| powerOffsetInformation:
| gainFactorInformation:
computedGainFactors (ReferenceTFC_ID): | 0
powerOffsetPp_m: | Omit
| :
ctfc4: | 8
| powerOffsetInformation:
| gainFactorInformation:
| signalledGainFactors:
| modeSpecificInfo:
| fdd:
gainFactorBetaC (GainFactor): | 11
gainFactorBetaD (GainFactor): | 15
referenceTFC_ID: | 0
powerOffsetPp_m: | Omit
| trCH_LogCHMapping: (TrCH_LogCHMappingList1)
| ulconnectedTrCHList: Omit
| dlconnectedTrCHList:
| :
trchid (TransportChannelIdentity): | 12
| trCH_LogCHMappingList:
| TrCH_LogicalChannelMapping:
| logicalChannel_Mapping:
| dl_LogicalChannelMapping: (SS_DL_LogicalChannelMapping)
macHeaderManipulation (MAC_HeaderManipulation): | normalMacHeader
dl_TransportChannelType (SS_DL_TransportChannelType): | pch
logicalChannelIdentity: | 1
logicalChannelType: | pCCH
| rlc_SizeList:
configured: |
mac_LogicalChannelPriority: | 1
rB_Identity: | -2
cn_DomainIdentity: | Omit
| :
trchid (TransportChannelIdentity): | 13
| trCH_LogCHMappingList:
| TrCH_LogicalChannelMapping:
| logicalChannel_Mapping:
| dl_LogicalChannelMapping: (SS_DL_LogicalChannelMapping)
macHeaderManipulation (MAC_HeaderManipulation): | normalMacHeader
dl_TransportChannelType (SS_DL_TransportChannelType): | fach
logicalChannelIdentity: | 6
logicalChannelType: | bCCH
| rlc_SizeList:
configured: |
mac_LogicalChannelPriority: | 6
rB_Identity: | -3
cn_DomainIdentity: | Omit
| TrCH_LogicalChannelMapping:
| logicalChannel_Mapping:
| dl_LogicalChannelMapping: (SS_DL_LogicalChannelMapping)
macHeaderManipulation (MAC_HeaderManipulation): | normalMacHeader
dl_TransportChannelType (SS_DL_TransportChannelType): | fach
logicalChannelIdentity: | 5
logicalChannelType: | cCCH
| rlc_SizeList:
configured: |
mac_LogicalChannelPriority: | 1
rB_Identity: | 0
cn_DomainIdentity: | Omit
| TrCH_LogicalChannelMapping:
| logicalChannel_Mapping:
| dl_LogicalChannelMapping: (SS_DL_LogicalChannelMapping)
macHeaderManipulation (MAC_HeaderManipulation): | normalMacHeader
dl_TransportChannelType (SS_DL_TransportChannelType): | fach
logicalChannelIdentity: | 1
logicalChannelType: | dCCH
| rlc_SizeList:
configured: |
mac_LogicalChannelPriority: | 1
rB_Identity: | 1
cn_DomainIdentity: | Omit
| TrCH_LogicalChannelMapping:
| logicalChannel_Mapping:
| dl_LogicalChannelMapping: (SS_DL_LogicalChannelMapping)
macHeaderManipulation (MAC_HeaderManipulation): | normalMacHeader
dl_TransportChannelType (SS_DL_TransportChannelType): | fach
logicalChannelIdentity: | 2
logicalChannelType: | dCCH
| rlc_SizeList:
configured: |
mac_LogicalChannelPriority: | 2
rB_Identity: | 2
cn_DomainIdentity: | Omit
| TrCH_LogicalChannelMapping:
| logicalChannel_Mapping:
| dl_LogicalChannelMapping: (SS_DL_LogicalChannelMapping)
macHeaderManipulation (MAC_HeaderManipulation): | normalMacHeader
dl_TransportChannelType (SS_DL_TransportChannelType): | fach
logicalChannelIdentity: | 3
logicalChannelType: | dCCH
| rlc_SizeList:
configured: |
mac_LogicalChannelPriority: | 3
rB_Identity: | 3
cn_DomainIdentity: | Omit
| TrCH_LogicalChannelMapping:
| logicalChannel_Mapping:
| dl_LogicalChannelMapping: (SS_DL_LogicalChannelMapping)
macHeaderManipulation (MAC_HeaderManipulation): | normalMacHeader
dl_TransportChannelType (SS_DL_TransportChannelType): | fach
logicalChannelIdentity: | 4
logicalChannelType: | dCCH
| rlc_SizeList:
configured: |
mac_LogicalChannelPriority: | 4
rB_Identity: | 4
cn_DomainIdentity: | Omit
| :
trchid (TransportChannelIdentity): | 14
| trCH_LogCHMappingList:
| TrCH_LogicalChannelMapping:
| logicalChannel_Mapping:
| dl_LogicalChannelMapping: (SS_DL_LogicalChannelMapping)
macHeaderManipulation (MAC_HeaderManipulation): | normalMacHeader
dl_TransportChannelType (SS_DL_TransportChannelType): | fach
logicalChannelIdentity: | 7
logicalChannelType: | dTCH
| rlc_SizeList:
configured: |
mac_LogicalChannelPriority: | 8
rB_Identity: | 20
cn_DomainIdentity: | Omit

#### CMAC_Config_CNF

LLA |  | RRC | @ 00:00:08.200

| Channel ID: |  | S-CCPCH#1
| Cell ID: |  | 0

| Message Details:
| CMAC_Config_CNF:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 5

#### CPHY_RL_Setup_REQ

RRC |  | LLA | @ 00:00:08.200

| Channel ID: |  | PICH#1
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_REQ:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 6
ratType: | fdd
| setupMessage: (CphyRlSetupReq)
| physicalChannelInfo:
| pICHInfo:
| pichinfo: (PICH_Info)
| fdd:
channelisationCode256: | 2
pi_CountPerFrame: | e18
sttd_Indicator: | false
dl_TxPower (PICH_PowerOffset): | -5
sccpchId_associated: | 5

#### CPHY Radio Link Setup REQ

LLA |  | PHY | @ 00:00:08.210

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: PICH
| CFN: |  | 62

| Message Details:
| Configuration Parameters:
Channel Offset: | 0
Scrambling Code: | 1600
Symbol Rate: | 15k
Channelization Code: | 2
Adjust Time: | 0
Power in dBm: | -53
Tx Diversity: | Off
NumOfDpdch: | 0
Np: | 18

#### CPHY Radio Link Setup CNF

PHY |  | LLA | @ 00:00:08.210

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: PICH
| CFN: |  | 62

| Message Details:

#### CPHY_RL_Setup_CNF

LLA |  | RRC | @ 00:00:08.220

| Channel ID: |  | PICH#1
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_CNF:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 6

#### CPHY_RL_Setup_REQ

RRC |  | LLA | @ 00:00:08.220

| Channel ID: |  | AICH#1
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_REQ:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 7
ratType: | fdd
| setupMessage: (CphyRlSetupReq)
| physicalChannelInfo:
| aICHInfo:
| aichinfo: (AICH_Info)
channelisationCode256: | 3
sttd_Indicator: | false
aich_TransmissionTiming: | e0
dl_TxPower (AICH_PowerOffset): | -5

#### CPHY Radio Link Setup REQ

LLA |  | PHY | @ 00:00:08.220

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: AICH
| CFN: |  | 63

| Message Details:
| Configuration Parameters:
Channel Offset: | 7680
Scrambling Code: | 1600
Symbol Rate: | 15k
Channelization Code: | 3
Adjust Time: | 0
Power in dBm: | -53
Tx Diversity: | Off
AICH Transmission Timing: | 3 Access Slots
AICH Polarity: | Positive
NumOfDpdch: | 0

#### CPHY Radio Link Setup CNF

PHY |  | LLA | @ 00:00:08.220

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: AICH
| CFN: |  | 63

| Message Details:

#### CPHY_RL_Setup_CNF

LLA |  | RRC | @ 00:00:08.230

| Channel ID: |  | AICH#1
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_CNF:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 7

#### CPHY_RL_Setup_REQ

RRC |  | LLA | @ 00:00:08.230

| Channel ID: |  | PRACH#1
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_REQ:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 8
ratType: | fdd
| setupMessage: (CphyRlSetupReq)
| physicalChannelInfo:
| pRACHInfo:
| fdd_tdd:
| fdd:
preambleSignature (AvailableSignatures): | 0000000011111111
spreadingFactorForDataPart (SF_PRACH): | sfpr64
preambleScramblingCode (PreambleScramblingCodeWordNumber): | 0
puncturingLimit: | pl1
accessSlot (AvailableSubChannelNumbers): | 111111111111

#### CPHY_RL_Setup_CNF

LLA |  | RRC | @ 00:00:08.250

| Channel ID: |  | PRACH#1
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_CNF:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 8

#### CPHY_TrCH_Config_REQ

RRC |  | LLA | @ 00:00:08.250

| Channel ID: |  | PRACH#1
| Cell ID: |  | 0

| Message Details:
| CPHY_TrCH_Config_REQ:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 8
ratType: | fdd
| trchConfigType:
nonDch: |
| configMessage: (CphyTrchConfigReq)
| activationTime: (SS_ActivationTime)
activateNow: |
| ulconnectedTrCHList:
| :
trchid (TransportChannelIdentity): | 15
ul_TransportChannelType (SS_UL_TransportChannelType): | rach
| transportChannelInfo: (CommonOrDedicatedTFS)
| tti:
| tti20: (CommonOrDedicatedTF_InfoList)
| CommonOrDedicatedTF_Info:
tb_Size: | 168
| numberOfTbSizeList:
| NumberOfTransportBlocks:
one: |
| logicalChannelList:
configured: |
| CommonOrDedicatedTF_Info:
tb_Size: | 360
| numberOfTbSizeList:
| NumberOfTransportBlocks:
one: |
| logicalChannelList:
configured: |
| semistaticTF_Information:
| channelCodingType:
convolutional (CodingRate): | half
rateMatchingAttribute: | 150
crc_Size: | crc16
| ulTFCS: (TFCS)
| normalTFCI_Signalling: (ExplicitTFCS_Configuration)
| complete: (TFCS_ReconfAdd)
| ctfcSize:
| ctfc2Bit:
| :
ctfc2: | 0
| powerOffsetInformation: Omit
| :
ctfc2: | 1
| powerOffsetInformation: Omit
| dlconnectedTrCHList: Omit
| dlTFCS: (TFCS) Omit

#### CPHY Radio Link Setup REQ

LLA |  | PHY | @ 00:00:08.260

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: PRACH
| CFN: |  | 67

| Message Details:
| Configuration Parameters:
Channel Offset: | 10240
Scrambling Code: | 16778816
Symbol Rate: | 60k
Channelization Code: | 128
Adjust Time: | 0
Slot Format: | 2
NumOfDpdch: | 1

#### CPHY Radio Link Setup CNF

PHY |  | LLA | @ 00:00:08.260

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: PRACH
| CFN: |  | 67

| Message Details:

#### CPHY Transport Channel Configuration REQ

LLA |  | PHY | @ 00:00:08.290

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: PRACH
| CFN: |  | 70

| Message Details:
| Configuration Parameters:
DTX Position: | Flexible
Second Interleave: | On
Puncture Limit: | 100
CCTrCH Length: | 600
Number Of Transport Channels: | 1
| Transport Channels:
| Item Number 0:
| Transport Channel Parameters:
| Transport Channel:
Name: | RACH
Identity: | 0
TTI (ms): | 20
EP Type: | 1/2 Rate Convolutional Coding
CRC Size: | 16
RM Attribute: | 150
First Interleave: | On
Number Of Transport Formats: | 2
| Transport Format Set:
| Transport Format 0:
Number Of Transport Blocks: | 1
Transport Block Size In Bits: | 168
| Transport Format 1:
Number Of Transport Blocks: | 1
Transport Block Size In Bits: | 360
RM Maximum Length: | 600
| Transport Format Combination Set:
Number Of Transport Format Combinations: | 2
| Transport Format Combinations 0:
Transport Format: | 0
| Transport Format Combinations 1:
Transport Format: | 1

#### CPHY Transport Channel Configuration CNF

PHY |  | LLA | @ 00:00:08.300

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: PRACH
| CFN: |  | 71

| Message Details:

#### CPHY_TrCH_Config_CNF

LLA |  | RRC | @ 00:00:08.310

| Channel ID: |  | PRACH#1
| Cell ID: |  | 0

| Message Details:
| CPHY_TrCH_Config_CNF:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 8

#### CMAC_Config_REQ

RRC |  | LLA | @ 00:00:08.310

| Channel ID: |  | PRACH#1
| Cell ID: |  | 0

| Message Details:
| CMAC_Config_REQ:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 8
ratType: | fdd
| configMessage:
| setup: (CmacConfigReq)
| activationTime: (SS_ActivationTime)
activateNow: |
| uE_Info:
| u_RNTI: Omit
c_RNTI: | 0000000000000001
| trCHInfo:
| ulconnectedTrCHList:
| :
trchid (TransportChannelIdentity): | 15
| transportChannelInfo: (CommonOrDedicatedTFS)
| tti:
| tti20: (CommonOrDedicatedTF_InfoList)
| CommonOrDedicatedTF_Info:
tb_Size: | 168
| numberOfTbSizeList:
| NumberOfTransportBlocks:
one: |
| logicalChannelList:
configured: |
| CommonOrDedicatedTF_Info:
tb_Size: | 360
| numberOfTbSizeList:
| NumberOfTransportBlocks:
one: |
| logicalChannelList:
configured: |
| semistaticTF_Information:
| channelCodingType:
convolutional (CodingRate): | half
rateMatchingAttribute: | 150
crc_Size: | crc16
| ulTFCS: (TFCS)
| normalTFCI_Signalling: (ExplicitTFCS_Configuration)
| complete: (TFCS_ReconfAdd)
| ctfcSize:
| ctfc2Bit:
| :
ctfc2: | 0
| powerOffsetInformation: Omit
| :
ctfc2: | 1
| powerOffsetInformation: Omit
| dlconnectedTrCHList: Omit
| dlTFCS: (TFCS) Omit
| trCH_LogCHMapping: (TrCH_LogCHMappingList1)
| ulconnectedTrCHList:
| :
trchid (TransportChannelIdentity): | 15
| trCH_LogCHMappingList:
| TrCH_LogicalChannelMapping:
| logicalChannel_Mapping:
| ul_LogicalChannelMapping: (SS_UL_LogicalChannelMapping)
macHeaderManipulation (MAC_HeaderManipulation): | normalMacHeader
ul_TransportChannelType (SS_UL_TransportChannelType): | rach
logicalChannelIdentity: | 5
logicalChannelType: | cCCH
rB_Identity: | 0
cn_DomainIdentity: | Omit
| TrCH_LogicalChannelMapping:
| logicalChannel_Mapping:
| ul_LogicalChannelMapping: (SS_UL_LogicalChannelMapping)
macHeaderManipulation (MAC_HeaderManipulation): | normalMacHeader
ul_TransportChannelType (SS_UL_TransportChannelType): | rach
logicalChannelIdentity: | 1
logicalChannelType: | dCCH
rB_Identity: | 1
cn_DomainIdentity: | Omit
| TrCH_LogicalChannelMapping:
| logicalChannel_Mapping:
| ul_LogicalChannelMapping: (SS_UL_LogicalChannelMapping)
macHeaderManipulation (MAC_HeaderManipulation): | normalMacHeader
ul_TransportChannelType (SS_UL_TransportChannelType): | rach
logicalChannelIdentity: | 2
logicalChannelType: | dCCH
rB_Identity: | 2
cn_DomainIdentity: | Omit
| TrCH_LogicalChannelMapping:
| logicalChannel_Mapping:
| ul_LogicalChannelMapping: (SS_UL_LogicalChannelMapping)
macHeaderManipulation (MAC_HeaderManipulation): | normalMacHeader
ul_TransportChannelType (SS_UL_TransportChannelType): | rach
logicalChannelIdentity: | 3
logicalChannelType: | dCCH
rB_Identity: | 3
cn_DomainIdentity: | Omit
| TrCH_LogicalChannelMapping:
| logicalChannel_Mapping:
| ul_LogicalChannelMapping: (SS_UL_LogicalChannelMapping)
macHeaderManipulation (MAC_HeaderManipulation): | normalMacHeader
ul_TransportChannelType (SS_UL_TransportChannelType): | rach
logicalChannelIdentity: | 4
logicalChannelType: | dCCH
rB_Identity: | 4
cn_DomainIdentity: | Omit
| TrCH_LogicalChannelMapping:
| logicalChannel_Mapping:
| ul_LogicalChannelMapping: (SS_UL_LogicalChannelMapping)
macHeaderManipulation (MAC_HeaderManipulation): | normalMacHeader
ul_TransportChannelType (SS_UL_TransportChannelType): | rach
logicalChannelIdentity: | 7
logicalChannelType: | dTCH
rB_Identity: | 20
cn_DomainIdentity: | Omit
| dlconnectedTrCHList: Omit

#### CMAC Configuration REQ

LLA |  | MAC | @ 00:00:08.320

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: PRACH
| CFN: |  | 73

| Message Details:
| Configuration Parameters:
Number Of Transport Channels: | 1
| Transport Channels:
| Item Number 0:
| Transport Channel Parameters:
| Transport Channel:
Name: | RACH
Identity: | 0
TTI (ms): | 20
EP Type: | 1/2 Rate Convolutional Coding
CRC Size: | 16
RM Attribute: | 150
First Interleave: | On
Number Of Transport Formats: | 2
| Transport Format Set:
| Transport Format 0:
Number Of Transport Blocks: | 1
Transport Block Size In Bits: | 168
| Transport Format 1:
Number Of Transport Blocks: | 1
Transport Block Size In Bits: | 360
Number Of Logical Channels: | 6
| Logical Channels:
| Item Number 0:
| Logical Channel:
Name: | CCCH
Identity: | 0
Priority: | 0
CT Length: | 0
CT Value: | 0
TCTF Length: | 2
TCTF Value: | 0
UE ID Type: | Not used
UE ID: | 0
| Item Number 1:
| Logical Channel:
Name: | DCCH
Identity: | 1
Priority: | 0
CT Length: | 4
CT Value: | 0
TCTF Length: | 2
TCTF Value: | 1
UE ID Type: | C RNTI
UE ID: | 1
| Item Number 2:
| Logical Channel:
Name: | DCCH
Identity: | 2
Priority: | 0
CT Length: | 4
CT Value: | 1
TCTF Length: | 2
TCTF Value: | 1
UE ID Type: | C RNTI
UE ID: | 1
| Item Number 3:
| Logical Channel:
Name: | DCCH
Identity: | 3
Priority: | 0
CT Length: | 4
CT Value: | 2
TCTF Length: | 2
TCTF Value: | 1
UE ID Type: | C RNTI
UE ID: | 1
| Item Number 4:
| Logical Channel:
Name: | DCCH
Identity: | 4
Priority: | 0
CT Length: | 4
CT Value: | 3
TCTF Length: | 2
TCTF Value: | 1
UE ID Type: | C RNTI
UE ID: | 1
| Item Number 5:
| Logical Channel:
Name: | U_DTCH
Identity: | 4
Priority: | 0
CT Length: | 4
CT Value: | 6
TCTF Length: | 2
TCTF Value: | 1
UE ID Type: | C RNTI
UE ID: | 1
Active Flag: | 1
| Transport Format Combination Set:
Number Of Transport Format Combinations: | 2
| Transport Format Combinations 0:
Transport Format: | 0
| Transport Format Combinations 1:
Transport Format: | 1

#### CMAC Configuration CNF

MAC |  | LLA | @ 00:00:08.320

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: PRACH
| CFN: |  | 73

| Message Details:

#### CMAC_Config_CNF

LLA |  | RRC | @ 00:00:08.340

| Channel ID: |  | PRACH#1
| Cell ID: |  | 0

| Message Details:
| CMAC_Config_CNF:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 8

#### CRLC_Config_REQ

RRC |  | LLA | @ 00:00:08.340

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CRLC_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CrlcConfigReq)
| setup: (RBInfo)
| sS_rlc_Info:
| sS_ul_RLC_Mode: (DL_RLC_Mode) Omit
| sS_dl_RLC_Mode:
dl_PayloadSize (PayloadSize): | 246
| dl_RLCModeInfo: (UL_RLC_Mode)
| ul_TM_RLC_Mode:
| transmissionRLC_Discard: Omit
segmentationIndication: | false
| rB_LogCH_Mapping:
uLlogicalChannelIdentity (LogicalChannelIdentity): | Omit
dLlogicalChannelIdentity (LogicalChannelIdentity): | 1
logicalChannelType: | Omit
cn_DomainIdentity: | Omit

#### CRLC TM Channel Establish REQ

LLA |  | RLC | @ 00:00:08.350

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCCH
| CFN: |  | 76

| Message Details:
| Configuration Parameters:
Number Of PU Sizes: | 1
| PU sizes In Bits:
Item 0: | 246

#### CRLC TM Channel Establish CNF

RLC |  | LLA | @ 00:00:08.350

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCCH
| CFN: |  | 76

| Message Details:

#### CRLC_Config_CNF

LLA |  | RRC | @ 00:00:08.360

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CRLC_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### CRLC_Config_REQ

RRC |  | LLA | @ 00:00:08.360

| Channel ID: |  | RbPcch
| Cell ID: |  | 0

| Message Details:
| CRLC_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -2
ratType: | fdd
| configMessage: (CrlcConfigReq)
| setup: (RBInfo)
| sS_rlc_Info:
| sS_ul_RLC_Mode: (DL_RLC_Mode) Omit
| sS_dl_RLC_Mode:
dl_PayloadSize (PayloadSize): | 240
| dl_RLCModeInfo: (UL_RLC_Mode)
| ul_TM_RLC_Mode:
| transmissionRLC_Discard: Omit
segmentationIndication: | false
| rB_LogCH_Mapping:
uLlogicalChannelIdentity (LogicalChannelIdentity): | Omit
dLlogicalChannelIdentity (LogicalChannelIdentity): | 1
logicalChannelType: | Omit
cn_DomainIdentity: | Omit

#### CRLC TM Channel Establish REQ

LLA |  | RLC | @ 00:00:08.360

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: PCCH
| CFN: |  | 77

| Message Details:
| Configuration Parameters:
Number Of PU Sizes: | 1
| PU sizes In Bits:
Item 0: | 240

#### CRLC TM Channel Establish CNF

RLC |  | LLA | @ 00:00:08.360

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: PCCH
| CFN: |  | 77

| Message Details:

#### CRLC_Config_CNF

LLA |  | RRC | @ 00:00:08.370

| Channel ID: |  | RbPcch
| Cell ID: |  | 0

| Message Details:
| CRLC_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -2

#### CRLC_Config_REQ

RRC |  | LLA | @ 00:00:08.370

| Channel ID: |  | Rb0
| Cell ID: |  | 0

| Message Details:
| CRLC_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | 0
ratType: | fdd
| configMessage: (CrlcConfigReq)
| setup: (RBInfo)
| sS_rlc_Info:
| sS_ul_RLC_Mode: (DL_RLC_Mode) Omit
| sS_dl_RLC_Mode:
dl_PayloadSize (PayloadSize): | 152
| dl_RLCModeInfo: (UL_RLC_Mode)
| ul_UM_RLC_Mode:
| transmissionRLC_Discard:
timerBasedNoExplicit (NoExplicitDiscard): | dt100
| rB_LogCH_Mapping:
uLlogicalChannelIdentity (LogicalChannelIdentity): | Omit
dLlogicalChannelIdentity (LogicalChannelIdentity): | 5
logicalChannelType: | Omit
cn_DomainIdentity: | Omit

#### CRLC UM Channel Establish REQ

LLA |  | RLC | @ 00:00:08.380

| BTS unit: |  | 1:1
| Channel No: |  | 1 Name: CCCH
| CFN: |  | 79

| Message Details:
| Configuration Parameters:
PU Size In Bits: | 152

#### CRLC UM Channel Establish CNF

RLC |  | LLA | @ 00:00:08.380

| BTS unit: |  | 1:1
| Channel No: |  | 1 Name: CCCH
| CFN: |  | 79

| Message Details:

#### CRLC_Config_CNF

LLA |  | RRC | @ 00:00:08.390

| Channel ID: |  | Rb0
| Cell ID: |  | 0

| Message Details:
| CRLC_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | 0

#### CRLC_Config_REQ

RRC |  | LLA | @ 00:00:08.390

| Channel ID: |  | Rb0
| Cell ID: |  | 0

| Message Details:
| CRLC_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | 0
ratType: | fdd
| configMessage: (CrlcConfigReq)
| setup: (RBInfo)
| sS_rlc_Info:
| sS_ul_RLC_Mode: (DL_RLC_Mode)
| dl_TM_RLC_Mode:
segmentationIndication: | false
| sS_dl_RLC_Mode:
dl_PayloadSize (PayloadSize): | 166
| dl_RLCModeInfo: (UL_RLC_Mode)
| ul_TM_RLC_Mode:
| transmissionRLC_Discard: Omit
segmentationIndication: | false
| rB_LogCH_Mapping:
uLlogicalChannelIdentity (LogicalChannelIdentity): | 5
dLlogicalChannelIdentity (LogicalChannelIdentity): | Omit
logicalChannelType: | Omit
cn_DomainIdentity: | Omit

#### CRLC_Config_CNF

LLA |  | RRC | @ 00:00:08.400

| Channel ID: |  | Rb0
| Cell ID: |  | 0

| Message Details:
| CRLC_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | 0

#### CRLC_Config_REQ

RRC |  | LLA | @ 00:00:08.400

| Channel ID: |  | Rb1
| Cell ID: |  | -1

| Message Details:
| CRLC_Config_REQ:
cellId: | -1
| routingInfo:
rB_Identity: | 1
ratType: | fdd
| configMessage: (CrlcConfigReq)
| setup: (RBInfo)
| sS_rlc_Info:
| sS_ul_RLC_Mode: (DL_RLC_Mode)
dl_UM_RLC_Mode: |
| sS_dl_RLC_Mode:
dl_PayloadSize (PayloadSize): | 136
| dl_RLCModeInfo: (UL_RLC_Mode)
| ul_UM_RLC_Mode:
| transmissionRLC_Discard:
timerBasedNoExplicit (NoExplicitDiscard): | dt100
| rB_LogCH_Mapping:
uLlogicalChannelIdentity (LogicalChannelIdentity): | 1
dLlogicalChannelIdentity (LogicalChannelIdentity): | 1
logicalChannelType: | Omit
cn_DomainIdentity: | Omit

#### CRLC TM Channel Establish REQ

LLA |  | RLC | @ 00:00:08.400

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: CCCH
| CFN: |  | 81

| Message Details:
| Configuration Parameters:
Number Of PU Sizes: | 1
| PU sizes In Bits:
Item 0: | 166

#### CRLC TM Channel Establish CNF

RLC |  | LLA | @ 00:00:08.400

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: CCCH
| CFN: |  | 81

| Message Details:

#### CRLC UM Channel Establish REQ

LLA |  | RLC | @ 00:00:08.410

| BTS unit: |  | 1:1
| Channel No: |  | 1 Name: DCCH
| CFN: |  | 82

| Message Details:
| Configuration Parameters:
PU Size In Bits: | 136

#### CRLC UM Channel Establish CNF

RLC |  | LLA | @ 00:00:08.410

| BTS unit: |  | 1:1
| Channel No: |  | 1 Name: DCCH
| CFN: |  | 82

| Message Details:

#### CRLC_Config_CNF

LLA |  | RRC | @ 00:00:08.420

| Channel ID: |  | Rb1
| Cell ID: |  | -1

| Message Details:
| CRLC_Config_CNF:
cellId: | -1
| routingInfo:
rB_Identity: | 1

#### CRLC_Config_REQ

RRC |  | LLA | @ 00:00:08.420

| Channel ID: |  | Rb2
| Cell ID: |  | -1

| Message Details:
| CRLC_Config_REQ:
cellId: | -1
| routingInfo:
rB_Identity: | 2
ratType: | fdd
| configMessage: (CrlcConfigReq)
| setup: (RBInfo)
| sS_rlc_Info:
| sS_ul_RLC_Mode: (DL_RLC_Mode)
| dl_AM_RLC_Mode:
inSequenceDelivery: | true
receivingWindowSize: | rw32
| dl_RLC_StatusInfo:
timerStatusProhibit: | tsp200
timerEPC: | Omit
missingPDU_Indicator: | true
timerStatusPeriodic: | Omit
| sS_dl_RLC_Mode:
dl_PayloadSize (PayloadSize): | 128
| dl_RLCModeInfo: (UL_RLC_Mode)
| ul_AM_RLC_Mode:
| transmissionRLC_Discard:
noDiscard (MaxDAT): | dat15
transmissionWindowSize: | tw32
timerRST: | tr500
max_RST (MaxRST): | rst1
| pollingInfo:
timerPollProhibit: | tpp200
timerPoll: | tp400
poll_PDU: | Omit
poll_SDU: | sdu1
lastTransmissionPDU_Poll: | true
lastRetransmissionPDU_Poll: | true
pollWindow: | pw99
timerPollPeriodic: | Omit
| rB_LogCH_Mapping:
uLlogicalChannelIdentity (LogicalChannelIdentity): | 2
dLlogicalChannelIdentity (LogicalChannelIdentity): | 2
logicalChannelType: | Omit
cn_DomainIdentity: | Omit

#### CRLC AM Channel Establish REQ

LLA |  | RLC | @ 00:00:08.430

| BTS unit: |  | 1:1
| Channel No: |  | 2 Name: DCCH
| CFN: |  | 84

| Message Details:
| Configuration Parameters:
PU Size In Bits: | 128
| Timer Parameters:
Poll (ms): | 400
Poll Prohibit (ms): | 0
EPC (ms): | 0
Discard (ms): | 0
Poll Periodic (ms): | 0
Status Prohibit (ms): | 0
Status Periodic (ms): | 0
Reset (ms): | 500
MRW (ms): | 0
| Protocol Parameters:
Max Dat: | 15
Poll PU: | 0
Poll SDU: | 1
Poll Window: | 99
Max Reset: | 1
Tx Window Size: | 32
Rx Window Size: | 32
Max MRW: | 0
SDU Discard Mode: | No discard
| Polling Triggers:
Last PU In Buffer: | On
Last PU In Retransmission Buffer: | On
Poll Timer: | On
Every Poll-PU PU: | Off
Every Poll-SDU SDU: | On
Poll-Window Percent Of Transmission Buffer: | On
Timer Based: | Off
| Status Triggers:
Missing PU: | On
Timer Based: | Off
EPC Mechanism: | Off

#### CRLC AM Channel Establish CNF

RLC |  | LLA | @ 00:00:08.430

| BTS unit: |  | 1:1
| Channel No: |  | 2 Name: DCCH
| CFN: |  | 84

| Message Details:

#### CRLC_Config_CNF

LLA |  | RRC | @ 00:00:08.440

| Channel ID: |  | Rb2
| Cell ID: |  | -1

| Message Details:
| CRLC_Config_CNF:
cellId: | -1
| routingInfo:
rB_Identity: | 2

#### CRLC_Config_REQ

RRC |  | LLA | @ 00:00:08.440

| Channel ID: |  | Rb3
| Cell ID: |  | -1

| Message Details:
| CRLC_Config_REQ:
cellId: | -1
| routingInfo:
rB_Identity: | 3
ratType: | fdd
| configMessage: (CrlcConfigReq)
| setup: (RBInfo)
| sS_rlc_Info:
| sS_ul_RLC_Mode: (DL_RLC_Mode)
| dl_AM_RLC_Mode:
inSequenceDelivery: | true
receivingWindowSize: | rw32
| dl_RLC_StatusInfo:
timerStatusProhibit: | tsp200
timerEPC: | Omit
missingPDU_Indicator: | true
timerStatusPeriodic: | Omit
| sS_dl_RLC_Mode:
dl_PayloadSize (PayloadSize): | 128
| dl_RLCModeInfo: (UL_RLC_Mode)
| ul_AM_RLC_Mode:
| transmissionRLC_Discard:
noDiscard (MaxDAT): | dat15
transmissionWindowSize: | tw32
timerRST: | tr500
max_RST (MaxRST): | rst1
| pollingInfo:
timerPollProhibit: | tpp200
timerPoll: | tp400
poll_PDU: | Omit
poll_SDU: | sdu1
lastTransmissionPDU_Poll: | true
lastRetransmissionPDU_Poll: | true
pollWindow: | pw99
timerPollPeriodic: | Omit
| rB_LogCH_Mapping:
uLlogicalChannelIdentity (LogicalChannelIdentity): | 3
dLlogicalChannelIdentity (LogicalChannelIdentity): | 3
logicalChannelType: | Omit
cn_DomainIdentity: | Omit

#### CRLC AM Channel Establish REQ

LLA |  | RLC | @ 00:00:08.440

| BTS unit: |  | 1:1
| Channel No: |  | 3 Name: DCCH
| CFN: |  | 85

| Message Details:
| Configuration Parameters:
PU Size In Bits: | 128
| Timer Parameters:
Poll (ms): | 400
Poll Prohibit (ms): | 0
EPC (ms): | 0
Discard (ms): | 0
Poll Periodic (ms): | 0
Status Prohibit (ms): | 0
Status Periodic (ms): | 0
Reset (ms): | 500
MRW (ms): | 0
| Protocol Parameters:
Max Dat: | 15
Poll PU: | 0
Poll SDU: | 1
Poll Window: | 99
Max Reset: | 1
Tx Window Size: | 32
Rx Window Size: | 32
Max MRW: | 0
SDU Discard Mode: | No discard
| Polling Triggers:
Last PU In Buffer: | On
Last PU In Retransmission Buffer: | On
Poll Timer: | On
Every Poll-PU PU: | Off
Every Poll-SDU SDU: | On
Poll-Window Percent Of Transmission Buffer: | On
Timer Based: | Off
| Status Triggers:
Missing PU: | On
Timer Based: | Off
EPC Mechanism: | Off

#### CRLC AM Channel Establish CNF

RLC |  | LLA | @ 00:00:08.440

| BTS unit: |  | 1:1
| Channel No: |  | 3 Name: DCCH
| CFN: |  | 85

| Message Details:

#### CRLC_Config_CNF

LLA |  | RRC | @ 00:00:08.450

| Channel ID: |  | Rb3
| Cell ID: |  | -1

| Message Details:
| CRLC_Config_CNF:
cellId: | -1
| routingInfo:
rB_Identity: | 3

#### CRLC_Config_REQ

RRC |  | LLA | @ 00:00:08.450

| Channel ID: |  | Rb4
| Cell ID: |  | -1

| Message Details:
| CRLC_Config_REQ:
cellId: | -1
| routingInfo:
rB_Identity: | 4
ratType: | fdd
| configMessage: (CrlcConfigReq)
| setup: (RBInfo)
| sS_rlc_Info:
| sS_ul_RLC_Mode: (DL_RLC_Mode)
| dl_AM_RLC_Mode:
inSequenceDelivery: | true
receivingWindowSize: | rw32
| dl_RLC_StatusInfo:
timerStatusProhibit: | tsp200
timerEPC: | Omit
missingPDU_Indicator: | true
timerStatusPeriodic: | Omit
| sS_dl_RLC_Mode:
dl_PayloadSize (PayloadSize): | 128
| dl_RLCModeInfo: (UL_RLC_Mode)
| ul_AM_RLC_Mode:
| transmissionRLC_Discard:
noDiscard (MaxDAT): | dat15
transmissionWindowSize: | tw32
timerRST: | tr500
max_RST (MaxRST): | rst1
| pollingInfo:
timerPollProhibit: | tpp200
timerPoll: | tp400
poll_PDU: | Omit
poll_SDU: | sdu1
lastTransmissionPDU_Poll: | true
lastRetransmissionPDU_Poll: | true
pollWindow: | pw99
timerPollPeriodic: | Omit
| rB_LogCH_Mapping:
uLlogicalChannelIdentity (LogicalChannelIdentity): | 4
dLlogicalChannelIdentity (LogicalChannelIdentity): | 4
logicalChannelType: | Omit
cn_DomainIdentity: | Omit

#### CRLC AM Channel Establish REQ

LLA |  | RLC | @ 00:00:08.460

| BTS unit: |  | 1:1
| Channel No: |  | 4 Name: DCCH
| CFN: |  | 87

| Message Details:
| Configuration Parameters:
PU Size In Bits: | 128
| Timer Parameters:
Poll (ms): | 400
Poll Prohibit (ms): | 0
EPC (ms): | 0
Discard (ms): | 0
Poll Periodic (ms): | 0
Status Prohibit (ms): | 0
Status Periodic (ms): | 0
Reset (ms): | 500
MRW (ms): | 0
| Protocol Parameters:
Max Dat: | 15
Poll PU: | 0
Poll SDU: | 1
Poll Window: | 99
Max Reset: | 1
Tx Window Size: | 32
Rx Window Size: | 32
Max MRW: | 0
SDU Discard Mode: | No discard
| Polling Triggers:
Last PU In Buffer: | On
Last PU In Retransmission Buffer: | On
Poll Timer: | On
Every Poll-PU PU: | Off
Every Poll-SDU SDU: | On
Poll-Window Percent Of Transmission Buffer: | On
Timer Based: | Off
| Status Triggers:
Missing PU: | On
Timer Based: | Off
EPC Mechanism: | Off

#### CRLC AM Channel Establish CNF

RLC |  | LLA | @ 00:00:08.460

| BTS unit: |  | 1:1
| Channel No: |  | 4 Name: DCCH
| CFN: |  | 87

| Message Details:

#### CRLC_Config_CNF

LLA |  | RRC | @ 00:00:08.470

| Channel ID: |  | Rb4
| Cell ID: |  | -1

| Message Details:
| CRLC_Config_CNF:
cellId: | -1
| routingInfo:
rB_Identity: | 4

#### CRLC_Config_REQ

RRC |  | LLA | @ 00:00:08.470

| Channel ID: |  | RbBcchFach
| Cell ID: |  | 0

| Message Details:
| CRLC_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -3
ratType: | fdd
| configMessage: (CrlcConfigReq)
| setup: (RBInfo)
| sS_rlc_Info:
| sS_ul_RLC_Mode: (DL_RLC_Mode) Omit
| sS_dl_RLC_Mode:
dl_PayloadSize (PayloadSize): | 166
| dl_RLCModeInfo: (UL_RLC_Mode)
| ul_TM_RLC_Mode:
| transmissionRLC_Discard: Omit
segmentationIndication: | true
| rB_LogCH_Mapping:
uLlogicalChannelIdentity (LogicalChannelIdentity): | Omit
dLlogicalChannelIdentity (LogicalChannelIdentity): | 6
logicalChannelType: | Omit
cn_DomainIdentity: | Omit

#### CRLC TM Channel Establish REQ

LLA |  | RLC | @ 00:00:08.470

| BTS unit: |  | 1:1
| Channel No: |  | 1 Name: BCCH
| CFN: |  | 88

| Message Details:
| Configuration Parameters:
Number Of PU Sizes: | 1
| PU sizes In Bits:
Item 0: | 166

#### CRLC TM Channel Establish CNF

RLC |  | LLA | @ 00:00:08.470

| BTS unit: |  | 1:1
| Channel No: |  | 1 Name: BCCH
| CFN: |  | 88

| Message Details:

#### CRLC_Config_CNF

LLA |  | RRC | @ 00:00:08.480

| Channel ID: |  | RbBcchFach
| Cell ID: |  | 0

| Message Details:
| CRLC_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -3

#### CRLC_Config_REQ

RRC |  | LLA | @ 00:00:08.480

| Channel ID: |  | Rb20
| Cell ID: |  | -1

| Message Details:
| CRLC_Config_REQ:
cellId: | -1
| routingInfo:
rB_Identity: | 20
ratType: | fdd
| configMessage: (CrlcConfigReq)
| setup: (RBInfo)
| sS_rlc_Info:
| sS_ul_RLC_Mode: (DL_RLC_Mode)
| dl_AM_RLC_Mode:
inSequenceDelivery: | true
receivingWindowSize: | rw128
| dl_RLC_StatusInfo:
timerStatusProhibit: | tsp200
timerEPC: | Omit
missingPDU_Indicator: | true
timerStatusPeriodic: | Omit
| sS_dl_RLC_Mode:
dl_PayloadSize (PayloadSize): | 320
| dl_RLCModeInfo: (UL_RLC_Mode)
| ul_AM_RLC_Mode:
| transmissionRLC_Discard:
noDiscard (MaxDAT): | dat15
transmissionWindowSize: | tw128
timerRST: | tr500
max_RST (MaxRST): | rst4
| pollingInfo:
timerPollProhibit: | tpp200
timerPoll: | tp400
poll_PDU: | Omit
poll_SDU: | sdu1
lastTransmissionPDU_Poll: | true
lastRetransmissionPDU_Poll: | true
pollWindow: | pw99
timerPollPeriodic: | Omit
| rB_LogCH_Mapping:
uLlogicalChannelIdentity (LogicalChannelIdentity): | 7
dLlogicalChannelIdentity (LogicalChannelIdentity): | 7
logicalChannelType: | Omit
cn_DomainIdentity: | Omit

#### CRLC AM Channel Establish REQ

LLA |  | RLC | @ 00:00:08.490

| BTS unit: |  | 1:1
| Channel No: |  | 4 Name: D_DTCH
| CFN: |  | 90

| Message Details:
| Configuration Parameters:
PU Size In Bits: | 320
| Timer Parameters:
Poll (ms): | 400
Poll Prohibit (ms): | 0
EPC (ms): | 0
Discard (ms): | 0
Poll Periodic (ms): | 0
Status Prohibit (ms): | 0
Status Periodic (ms): | 0
Reset (ms): | 500
MRW (ms): | 0
| Protocol Parameters:
Max Dat: | 15
Poll PU: | 0
Poll SDU: | 1
Poll Window: | 99
Max Reset: | 4
Tx Window Size: | 128
Rx Window Size: | 128
Max MRW: | 0
SDU Discard Mode: | No discard
| Polling Triggers:
Last PU In Buffer: | On
Last PU In Retransmission Buffer: | On
Poll Timer: | On
Every Poll-PU PU: | Off
Every Poll-SDU SDU: | On
Poll-Window Percent Of Transmission Buffer: | On
Timer Based: | Off
| Status Triggers:
Missing PU: | On
Timer Based: | Off
EPC Mechanism: | Off

#### CRLC AM Channel Establish CNF

RLC |  | LLA | @ 00:00:08.490

| BTS unit: |  | 1:1
| Channel No: |  | 4 Name: D_DTCH
| CFN: |  | 90

| Message Details:

#### CRLC_Config_CNF

LLA |  | RRC | @ 00:00:08.500

| Channel ID: |  | Rb20
| Cell ID: |  | -1

| Message Details:
| CRLC_Config_CNF:
cellId: | -1
| routingInfo:
rB_Identity: | 20

#### o_SIB_PER_Encoding

RRC |  | RRC | @ 00:00:08.510

| Category: |  | TSO

| Message Details:
| Inputs:
| SIB:
| sIB1: (SysInfoType1)
cn_CommonGSM_MAP_NAS_SysInfo (NAS_SystemInformationGSM_MAP): |
[0] | 00 | 01 |  |  |  |  |  |
| cn_DomainSysInfoList:
| CN_DomainSysInfo:
cn_DomainIdentity: | ps_domain
| cn_Type:
gsm_MAP (NAS_SystemInformationGSM_MAP): |
[0] | 01 | 00 |  |  |  |  |  |
cn_DRX_CycleLengthCoeff (CN_DRX_CycleLengthCoefficient): | 7
| CN_DomainSysInfo:
cn_DomainIdentity: | cs_domain
| cn_Type:
gsm_MAP (NAS_SystemInformationGSM_MAP): |
[0] | 1E | 01 |  |  |  |  |  |
cn_DRX_CycleLengthCoeff (CN_DRX_CycleLengthCoefficient): | 7
| ue_ConnTimersAndConstants:
t_301: | ms2000
n_301: | 2
t_302: | ms4000
n_302: | 3
t_304: | ms1000
n_304: | 3
t_305: | m60
t_307: | s50
t_308: | ms320
t_309: | 8
t_310: | ms320
n_310: | 5
t_311: | ms500
t_312: | 5
n_312: | s200
t_313: | 10
n_313: | s20
t_314: | s20
t_315: | s30
n_315: | s200
t_316: | s50
t_317: | s1800
| ue_IdleTimersAndConstants:
t_300: | ms4000
n_300: | 7
t_312: | 10
n_312: | s200
| v3a0NonCriticalExtensions: Omit
| Outputs:
BITSTRING: |
[0] | 11 | 00 | 01 | 00 | 00 | 00 | 00 | 00
[8] | 00 | 00 | 01 | 01 | 10 | 00 | 10 | 00
[16] | 00 | 00 | 10 | 00 | 00 | 00 | 00 | 10
[24] | 00 | 01 | 00 | 01 | 11 | 10 | 00 | 00
[32] | 00 | 01 | 01 | 00 | 00 | 11 | 11 | 11
[40] | 11 | 11 | 11 | 01 | 11 | 11 | 01 | 10
[48] | 11 | 10 | 01 | 10 | 11 | 11 | 11 | 11
[56] | 10 | 10 | 01 | 01 | 01 | 01 | 11 | 01
[64] | 01 | 11 | 01 | 00 | 11 | 10 | 11 | 11
[72] | 11 | 00 | 11 | 11 | 01 | 00 | 11 |

#### o_SIB_PER_Encoding

RRC |  | RRC | @ 00:00:08.510

| Category: |  | TSO

| Message Details:
| Inputs:
| SIB:
| sIB2: (SysInfoType2)
| ura_IdentityList:
URA_Identity: | 0000000000000001
| nonCriticalExtensions: Omit
| Outputs:
BITSTRING: |
[0] | 00 | 00 | 00 | 00 | 00 | 00 | 00 | 00
[8] | 00 | 01 |  |  |  |  |  |

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:08.510

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 10
bcch_ModificationTime: | Omit

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:08.530

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:08.530

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
| completeSIB_List:
| CompleteSIBshort:
sib_Type: | systemInformationBlockType1
sib_Data_variable: | 11000100000000000000010110001000000010000000001000010001111000000001010000111111111111011111011011100110111111111010010101011101011101001110111111001111010011
| CompleteSIBshort:
sib_Type: | systemInformationBlockType2
sib_Data_variable: | 00000000000000000001

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA |  | RLC | @ 00:00:08.530

| Channel No: |  | 0 Name: BCCH

| Message Details:
| SIB repetition rate: 64
| SIB position: 20
| BCCH_BCH_Message:
| message:
| sfn_Prime: 0
| payload:
| completeSIB_List:
| CompleteSIB_List.element:
| sib_Type: systemInformationBlockType1_SIB_Type [enum=1]
| sib_Data_variable: 11000100000000000000010110001000000010000000001000010001111000000001010000111111111111011111011011100110111111111010010101011101011101001110111111001111010011
| CompleteSIB_List.element:
| sib_Type: systemInformationBlockType2_SIB_Type [enum=2]
| sib_Data_variable: 00000000000000000001
Layer 3 SDU: |
[0] | 00 | 0E | 21 | 9D | C4 | 00 | 05 | 88
[8] | 08 | 02 | 11 | E0 | 14 | 3F | FD | F6
[16] | E6 | FF | A5 | 5D | 74 | EF | CF | 4C
[24] | 42 | 60 | 00 | 02 |  |  |  |

#### o_SIB_PER_Encoding

RRC |  | RRC | @ 00:00:08.530

| Category: |  | TSO

| Message Details:
| Inputs:
| SIB:
| sIB2: (SysInfoType2)
| ura_IdentityList:
URA_Identity: | 0000000000000001
| nonCriticalExtensions: Omit
| Outputs:
BITSTRING: |
[0] | 00 | 00 | 00 | 00 | 00 | 00 | 00 | 00
[8] | 00 | 01 |  |  |  |  |  |

#### o_SIB_PER_Encoding

RRC |  | RRC | @ 00:00:08.530

| Category: |  | TSO

| Message Details:
| Inputs:
| SIB:
| sIB1: (SysInfoType1)
cn_CommonGSM_MAP_NAS_SysInfo (NAS_SystemInformationGSM_MAP): |
[0] | 00 | 01 |  |  |  |  |  |
| cn_DomainSysInfoList:
| CN_DomainSysInfo:
cn_DomainIdentity: | ps_domain
| cn_Type:
gsm_MAP (NAS_SystemInformationGSM_MAP): |
[0] | 01 | 00 |  |  |  |  |  |
cn_DRX_CycleLengthCoeff (CN_DRX_CycleLengthCoefficient): | 7
| CN_DomainSysInfo:
cn_DomainIdentity: | cs_domain
| cn_Type:
gsm_MAP (NAS_SystemInformationGSM_MAP): |
[0] | 1E | 01 |  |  |  |  |  |
cn_DRX_CycleLengthCoeff (CN_DRX_CycleLengthCoefficient): | 7
| ue_ConnTimersAndConstants:
t_301: | ms2000
n_301: | 2
t_302: | ms4000
n_302: | 3
t_304: | ms1000
n_304: | 3
t_305: | m60
t_307: | s50
t_308: | ms320
t_309: | 8
t_310: | ms320
n_310: | 5
t_311: | ms500
t_312: | 5
n_312: | s200
t_313: | 10
n_313: | s20
t_314: | s20
t_315: | s30
n_315: | s200
t_316: | s50
t_317: | s1800
| ue_IdleTimersAndConstants:
t_300: | ms4000
n_300: | 7
t_312: | 10
n_312: | s200
| v3a0NonCriticalExtensions: Omit
| Outputs:
BITSTRING: |
[0] | 11 | 00 | 01 | 00 | 00 | 00 | 00 | 00
[8] | 00 | 00 | 01 | 01 | 10 | 00 | 10 | 00
[16] | 00 | 00 | 10 | 00 | 00 | 00 | 00 | 10
[24] | 00 | 01 | 00 | 01 | 11 | 10 | 00 | 00
[32] | 00 | 01 | 01 | 00 | 00 | 11 | 11 | 11
[40] | 11 | 11 | 11 | 01 | 11 | 11 | 01 | 10
[48] | 11 | 10 | 01 | 10 | 11 | 11 | 11 | 11
[56] | 10 | 10 | 01 | 01 | 01 | 01 | 11 | 01
[64] | 01 | 11 | 01 | 00 | 11 | 10 | 11 | 11
[72] | 11 | 00 | 11 | 11 | 01 | 00 | 11 |

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:08.530

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 10
bcch_ModificationTime: | Omit

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:08.540

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:08.540

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
| completeSIB_List:
| CompleteSIBshort:
sib_Type: | systemInformationBlockType1
sib_Data_variable: | 11000100000000000000010110001000000010000000001000010001111000000001010000111111111111011111011011100110111111111010010101011101011101001110111111001111010011
| CompleteSIBshort:
sib_Type: | systemInformationBlockType2
sib_Data_variable: | 00000000000000000001

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA |  | RLC | @ 00:00:08.540

| Channel No: |  | 0 Name: BCCH

| Message Details:
| SIB repetition rate: 64
| SIB position: 20
| BCCH_BCH_Message:
| message:
| sfn_Prime: 0
| payload:
| completeSIB_List:
| CompleteSIB_List.element:
| sib_Type: systemInformationBlockType1_SIB_Type [enum=1]
| sib_Data_variable: 11000100000000000000010110001000000010000000001000010001111000000001010000111111111111011111011011100110111111111010010101011101011101001110111111001111010011
| CompleteSIB_List.element:
| sib_Type: systemInformationBlockType2_SIB_Type [enum=2]
| sib_Data_variable: 00000000000000000001
Layer 3 SDU: |
[0] | 00 | 0E | 21 | 9D | C4 | 00 | 05 | 88
[8] | 08 | 02 | 11 | E0 | 14 | 3F | FD | F6
[16] | E6 | FF | A5 | 5D | 74 | EF | CF | 4C
[24] | 42 | 60 | 00 | 02 |  |  |  |

#### MAC_DATA_REQ

RLC |  | MAC | @ 00:00:08.550

| Category: |  | Configuration
| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCCH
| CFN: |  | 96

| Message Details:
RLC PDU size (bits): | 224
RLC PDU (raw): |
[0] | 00 | 0E | 21 | 9D | C4 | 00 | 05 | 88
[8] | 08 | 02 | 11 | E0 | 14 | 3F | FD | F6
[16] | E6 | FF | A5 | 5D | 74 | EF | CF | 4C
[24] | 42 | 60 | 00 | 02 |  |  |  |

#### PHY_DATA_REQ

MAC |  | PHY | @ 00:00:08.550

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCH
| CFN: |  | 96

| Message Details:
SIB repetition period: | 64
SIB position: | 20
SIB size: | 246
SIB (raw): |
[0] | 00 | 0E | 21 | 9D | C4 | 00 | 05 | 88
[8] | 08 | 02 | 11 | E0 | 14 | 3F | FD | F6
[16] | E6 | FF | A5 | 5D | 74 | EF | CF | 4C
[24] | 42 | 60 | 00 | 02 | 00 | 00 | 00 | 00
| SIB (decoded):
| TB 0:
MAC SDU (246 bits): |
[0] | 00 | 0E | 21 | 9D | C4 | 00 | 05 | 88
[8] | 08 | 02 | 11 | E0 | 14 | 3F | FD | F6
[16] | E6 | FF | A5 | 5D | 74 | EF | CF | 4C
[24] | 42 | 60 | 00 | 02 | 00 | 00 | 00 |

#### o_SIB_PER_Encoding

RRC |  | RRC | @ 00:00:08.560

| Category: |  | TSO

| Message Details:
| Inputs:
| SIB:
| sIB3: (SysInfoType3)
sib4indicator: | true
cellIdentity: | 0000000000000000000000000000
| cellSelectReselectInfo: (CellSelectReselectInfoSIB_3_4)
| mappingInfo: Omit
| cellSelectQualityMeasure:
cpich_RSCP: |
| modeSpecificInfo:
| fdd:
s_Intrasearch (S_SearchQual): | 8
s_Intersearch (S_SearchQual): | 8
s_SearchHCS (S_SearchRXLEV): | Omit
| rat_List: (RAT_FDD_InfoList)
| RAT_FDD_Info:
rat_Identifier: | gsm
s_SearchRAT (S_SearchQual): | -16
s_HCS_RAT (S_SearchRXLEV): | Omit
s_Limit_SearchRAT (S_SearchQual): | 0
q_QualMin: | -24
q_RxlevMin: | -40
q_Hyst_l_S (Q_Hyst_S): | 2
t_Reselection_S: | 0
| hcs_ServingCellInformation: Omit
maxAllowedUL_TX_Power: | 21
| cellAccessRestriction:
| cellBarred:
notBarred: |
cellReservedForOperatorUse (ReservedIndicator): | notReserved
cellReservationExtension (ReservedIndicator): | notReserved
| accessClassBarredList:
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
| nonCriticalExtensions: Omit
| Outputs:
BITSTRING: |
[0] | 01 | 00 | 00 | 00 | 00 | 00 | 00 | 00
[8] | 00 | 00 | 00 | 00 | 00 | 00 | 00 | 00
[16] | 10 | 11 | 01 | 11 | 00 | 01 | 10 | 00
[24] | 00 | 00 | 00 | 00 | 00 | 01 | 00 | 00
[32] | 00 | 00 | 00 | 10 | 01 | 00 | 00 | 10
[40] | 00 | 00 | 01 | 00 | 01 | 11 | 11 | 11
[48] | 11 | 11 | 11 | 11 | 11 | 11 | 11 | 11

#### o_SIB_PER_Encoding

RRC |  | RRC | @ 00:00:08.560

| Category: |  | TSO

| Message Details:
| Inputs:
| SIB:
| sIB7: (SysInfoType7)
| modeSpecificInfo:
| fdd:
ul_Interference: | -100
| prach_Information_SIB5_List: (DynamicPersistenceLevelList)
DynamicPersistenceLevel: | 2
| prach_Information_SIB6_List: (DynamicPersistenceLevelList)
DynamicPersistenceLevel: | 2
expirationTimeFactor: | Omit
| nonCriticalExtensions: Omit
| Outputs:
BITSTRING: |
[0] | 10 | 00 | 00 | 10 | 10 | 00 | 00 | 00
[8] | 10 | 00 | 00 | 01 |  |  |  |

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:08.560

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 7
bcch_ModificationTime: | Omit

#### MAC_DATA_REQ

RLC |  | MAC | @ 00:00:08.560

| Category: |  | Configuration
| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCCH
| CFN: |  | 97

| Message Details:
RLC PDU size (bits): | 224
RLC PDU (raw): |
[0] | 00 | 0E | 21 | 9D | C4 | 00 | 05 | 88
[8] | 08 | 02 | 11 | E0 | 14 | 3F | FD | F6
[16] | E6 | FF | A5 | 5D | 74 | EF | CF | 4C
[24] | 42 | 60 | 00 | 02 |  |  |  |

#### PHY_DATA_REQ

MAC |  | PHY | @ 00:00:08.570

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCH
| CFN: |  | 98

| Message Details:
SIB repetition period: | 64
SIB position: | 20
SIB size: | 246
SIB (raw): |
[0] | 00 | 0E | 21 | 9D | C4 | 00 | 05 | 88
[8] | 08 | 02 | 11 | E0 | 14 | 3F | FD | F6
[16] | E6 | FF | A5 | 5D | 74 | EF | CF | 4C
[24] | 42 | 60 | 00 | 02 | 00 | 00 | 00 | 00
| SIB (decoded):
| TB 0:
MAC SDU (246 bits): |
[0] | 00 | 0E | 21 | 9D | C4 | 00 | 05 | 88
[8] | 08 | 02 | 11 | E0 | 14 | 3F | FD | F6
[16] | E6 | FF | A5 | 5D | 74 | EF | CF | 4C
[24] | 42 | 60 | 00 | 02 | 00 | 00 | 00 |

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:08.580

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:08.580

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
| completeSIB_List:
| CompleteSIBshort:
sib_Type: | systemInformationBlockType7
sib_Data_variable: | 100000101000000010000001
| CompleteSIBshort:
sib_Type: | systemInformationBlockType3
sib_Data_variable: | 0100000000000000000000000000000010110111000110000000000000010000000000100100001000000100011111111111111111111111

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA |  | RLC | @ 00:00:08.580

| Channel No: |  | 0 Name: BCCH

| Message Details:
| SIB repetition rate: 64
| SIB position: 14
| BCCH_BCH_Message:
| message:
| sfn_Prime: 0
| payload:
| completeSIB_List:
| CompleteSIB_List.element:
| sib_Type: systemInformationBlockType7_SIB_Type [enum=7]
| sib_Data_variable: 100000101000000010000001
| CompleteSIB_List.element:
| sib_Type: systemInformationBlockType3_SIB_Type [enum=3]
| sib_Data_variable: 0100000000000000000000000000000010110111000110000000000000010000000000100100001000000100011111111111111111111111
Layer 3 SDU: |
[0] | 00 | 0E | 27 | 17 | 82 | 80 | 81 | 1B
[8] | 7A | 00 | 00 | 00 | 05 | B8 | C0 | 00
[16] | 80 | 12 | 10 | 23 | FF | FF | F8 |

#### o_SIB_PER_Encoding

RRC |  | RRC | @ 00:00:08.580

| Category: |  | TSO

| Message Details:
| Inputs:
| SIB:
| sIB4: (SysInfoType4)
cellIdentity: | 0000000000000000000000000000
| cellSelectReselectInfo: (CellSelectReselectInfoSIB_3_4)
| mappingInfo: Omit
| cellSelectQualityMeasure:
cpich_RSCP: |
| modeSpecificInfo:
| fdd:
s_Intrasearch (S_SearchQual): | 8
s_Intersearch (S_SearchQual): | 8
s_SearchHCS (S_SearchRXLEV): | Omit
| rat_List: (RAT_FDD_InfoList)
| RAT_FDD_Info:
rat_Identifier: | gsm
s_SearchRAT (S_SearchQual): | -16
s_HCS_RAT (S_SearchRXLEV): | Omit
s_Limit_SearchRAT (S_SearchQual): | 0
q_QualMin: | -24
q_RxlevMin: | -40
q_Hyst_l_S (Q_Hyst_S): | 0
t_Reselection_S: | 0
| hcs_ServingCellInformation: Omit
maxAllowedUL_TX_Power: | 21
| cellAccessRestriction:
| cellBarred:
notBarred: |
cellReservedForOperatorUse (ReservedIndicator): | notReserved
cellReservationExtension (ReservedIndicator): | notReserved
| accessClassBarredList: Omit
| nonCriticalExtensions: Omit
| Outputs:
BITSTRING: |
[0] | 00 | 00 | 00 | 00 | 00 | 00 | 00 | 00
[8] | 00 | 00 | 00 | 00 | 00 | 00 | 00 | 01
[16] | 01 | 10 | 11 | 10 | 00 | 11 | 00 | 00
[24] | 00 | 00 | 00 | 00 | 00 | 10 | 00 | 00
[32] | 00 | 00 | 01 | 00 | 10 | 00 | 00 | 00
[40] | 00 | 00 | 10 | 00 | 11 | 10 | 11 | 1

#### o_SIB_PER_Encoding

RRC |  | RRC | @ 00:00:08.580

| Category: |  | TSO

| Message Details:
| Inputs:
| SIB:
| sIB7: (SysInfoType7)
| modeSpecificInfo:
| fdd:
ul_Interference: | -100
| prach_Information_SIB5_List: (DynamicPersistenceLevelList)
DynamicPersistenceLevel: | 2
| prach_Information_SIB6_List: (DynamicPersistenceLevelList)
DynamicPersistenceLevel: | 2
expirationTimeFactor: | Omit
| nonCriticalExtensions: Omit
| Outputs:
BITSTRING: |
[0] | 10 | 00 | 00 | 10 | 10 | 00 | 00 | 00
[8] | 10 | 00 | 00 | 01 |  |  |  |

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:08.580

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 31
bcch_ModificationTime: | Omit

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:08.590

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:08.590

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
| completeSIB_List:
| CompleteSIBshort:
sib_Type: | systemInformationBlockType7
sib_Data_variable: | 100000101000000010000001
| CompleteSIBshort:
sib_Type: | systemInformationBlockType4
sib_Data_variable: | 00000000000000000000000000000001011011100011000000000000001000000000010010000000000010001110111

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA |  | RLC | @ 00:00:08.590

| Channel No: |  | 0 Name: BCCH

| Message Details:
| SIB repetition rate: 64
| SIB position: 62
| BCCH_BCH_Message:
| message:
| sfn_Prime: 0
| payload:
| completeSIB_List:
| CompleteSIB_List.element:
| sib_Type: systemInformationBlockType7_SIB_Type [enum=7]
| sib_Data_variable: 100000101000000010000001
| CompleteSIB_List.element:
| sib_Type: systemInformationBlockType4_SIB_Type [enum=4]
| sib_Data_variable: 00000000000000000000000000000001011011100011000000000000001000000000010010000000000010001110111
Layer 3 SDU: |
[0] | 00 | 0E | 27 | 17 | 82 | 80 | 81 | 22
[8] | F0 | 00 | 00 | 00 | 0B | 71 | 80 | 01
[16] | 00 | 24 | 00 | 47 | 70 |  |  |

#### o_SIB_PER_Encoding

RRC |  | RRC | @ 00:00:08.610

| Category: |  | TSO

| Message Details:
| Inputs:
| SIB:
| sIB5: (SysInfoType5)
sib6indicator: | true
pich_PowerOffset: | -5
| modeSpecificInfo:
| fdd:
aich_PowerOffset: | -5
| primaryCCPCH_Info: Omit
| prach_SystemInformationList:
| PRACH_SystemInformation:
| prach_RACH_Info:
| modeSpecificInfo:
| fdd:
availableSignatures: | 0000000011111111
availableSF (SF_PRACH): | sfpr64
preambleScramblingCodeWordNumber: | 0
puncturingLimit: | pl1
availableSubChannelNumbers: | 111111111111
transportChannelIdentity: | 15
| rach_TransportFormatSet: (TransportFormatSet)
| commonTransChTFS:
| tti:
| tti20: (CommonDynamicTF_InfoList)
| CommonDynamicTF_Info:
| rlc_Size:
| fdd:
| octetModeRLC_SizeInfoType2:
sizeType1: | 15
| numberOfTbSizeList:
| NumberOfTransportBlocks:
one: |
| logicalChannelList:
configured: |
| CommonDynamicTF_Info:
| rlc_Size:
| fdd:
| octetModeRLC_SizeInfoType2:
sizeType2: | 3
| numberOfTbSizeList:
| NumberOfTransportBlocks:
one: |
| logicalChannelList:
configured: |
| semistaticTF_Information:
| channelCodingType:
convolutional (CodingRate): | half
rateMatchingAttribute: | 150
crc_Size: | crc16
| rach_TFCS: (TFCS)
| normalTFCI_Signalling: (ExplicitTFCS_Configuration)
| complete: (TFCS_ReconfAdd)
| ctfcSize:
| ctfc2Bit:
| :
ctfc2: | 0
| powerOffsetInformation:
| gainFactorInformation:
computedGainFactors (ReferenceTFC_ID): | 0
powerOffsetPp_m: | 0
| :
ctfc2: | 1
| powerOffsetInformation:
| gainFactorInformation:
| signalledGainFactors:
| modeSpecificInfo:
| fdd:
gainFactorBetaC (GainFactor): | 11
gainFactorBetaD (GainFactor): | 15
referenceTFC_ID: | 0
powerOffsetPp_m: | 0
| prach_Partitioning:
| fdd:
| ASCSetting_FDD:
| accessServiceClass_FDD: Omit
| ASCSetting_FDD:
| accessServiceClass_FDD:
availableSignatureStartIndex: | 0
availableSignatureEndIndex: | 7
assignedSubChannelNumber: | 1111
| ASCSetting_FDD:
| accessServiceClass_FDD: Omit
| ASCSetting_FDD:
| accessServiceClass_FDD:
availableSignatureStartIndex: | 0
availableSignatureEndIndex: | 7
assignedSubChannelNumber: | 1111
| ASCSetting_FDD:
| accessServiceClass_FDD: Omit
| ASCSetting_FDD:
| accessServiceClass_FDD:
availableSignatureStartIndex: | 0
availableSignatureEndIndex: | 7
assignedSubChannelNumber: | 1111
| ASCSetting_FDD:
| accessServiceClass_FDD: Omit
| ASCSetting_FDD:
| accessServiceClass_FDD:
availableSignatureStartIndex: | 0
availableSignatureEndIndex: | 7
assignedSubChannelNumber: | 1111
| persistenceScalingFactorList:
PersistenceScalingFactor: | psf0_9
PersistenceScalingFactor: | psf0_9
PersistenceScalingFactor: | psf0_9
PersistenceScalingFactor: | psf0_9
PersistenceScalingFactor: | psf0_9
PersistenceScalingFactor: | psf0_9
| ac_To_ASC_MappingTable:
AC_To_ASC_Mapping: | 6
AC_To_ASC_Mapping: | 5
AC_To_ASC_Mapping: | 4
AC_To_ASC_Mapping: | 3
AC_To_ASC_Mapping: | 2
AC_To_ASC_Mapping: | 1
AC_To_ASC_Mapping: | 0
| modeSpecificInfo:
| fdd:
primaryCPICH_TX_Power: | 31
constantValue: | -10
| prach_PowerOffset:
powerRampStep: | 3
preambleRetransMax: | 4
| rach_TransmissionParameters:
mmax: | 2
nb01Min (NB01): | 3
nb01Max (NB01): | 10
| aich_Info:
channelisationCode256: | 3
sttd_Indicator: | false
aich_TransmissionTiming: | e0
| sCCPCH_SystemInformationList:
| SCCPCH_SystemInformation:
| secondaryCCPCH_Info:
| modeSpecificInfo:
| fdd:
dummy1 (PCPICH_UsageForChannelEst): | mayBeUsed
| dummy2: (SecondaryCPICH_Info) Omit
secondaryScramblingCode: | Omit
sttd_Indicator: | false
| sf_AndCodeNumber: (SF256_AndCodeNumber)
sf64: | 1
pilotSymbolExistence: | false
tfci_Existence: | true
positionFixedOrFlexible: | flexible
timingOffset: | 0
| tfcs:
| normalTFCI_Signalling: (ExplicitTFCS_Configuration)
| complete: (TFCS_ReconfAdd)
| ctfcSize:
| ctfc4Bit:
| :
ctfc4: | 0
| powerOffsetInformation: Omit
| :
ctfc4: | 1
| powerOffsetInformation: Omit
| :
ctfc4: | 2
| powerOffsetInformation: Omit
| :
ctfc4: | 3
| powerOffsetInformation: Omit
| :
ctfc4: | 4
| powerOffsetInformation: Omit
| :
ctfc4: | 5
| powerOffsetInformation: Omit
| :
ctfc4: | 6
| powerOffsetInformation: Omit
| :
ctfc4: | 8
| powerOffsetInformation: Omit
| fach_PCH_InformationList:
| FACH_PCH_Information:
| transportFormatSet:
| commonTransChTFS:
| tti:
| tti10: (CommonDynamicTF_InfoList)
| CommonDynamicTF_Info:
| rlc_Size:
| fdd:
| octetModeRLC_SizeInfoType2:
sizeType1: | 24
| numberOfTbSizeList:
| NumberOfTransportBlocks:
zero: |
| NumberOfTransportBlocks:
one: |
| logicalChannelList:
allSizes: |
| semistaticTF_Information:
| channelCodingType:
convolutional (CodingRate): | half
rateMatchingAttribute: | 230
crc_Size: | crc16
transportChannelIdentity: | 12
ctch_Indicator: | false
| FACH_PCH_Information:
| transportFormatSet:
| commonTransChTFS:
| tti:
| tti10: (CommonDynamicTF_InfoList)
| CommonDynamicTF_Info:
| rlc_Size:
| fdd:
| octetModeRLC_SizeInfoType2:
sizeType1: | 15
| numberOfTbSizeList:
| NumberOfTransportBlocks:
zero: |
| NumberOfTransportBlocks:
one: |
| NumberOfTransportBlocks:
small: | 2
| logicalChannelList:
allSizes: |
| semistaticTF_Information:
| channelCodingType:
convolutional (CodingRate): | half
rateMatchingAttribute: | 220
crc_Size: | crc16
transportChannelIdentity: | 13
ctch_Indicator: | false
| FACH_PCH_Information:
| transportFormatSet:
| commonTransChTFS:
| tti:
| tti10: (CommonDynamicTF_InfoList)
| CommonDynamicTF_Info:
| rlc_Size:
| fdd:
| octetModeRLC_SizeInfoType2:
sizeType2: | 3
| numberOfTbSizeList:
| NumberOfTransportBlocks:
zero: |
| NumberOfTransportBlocks:
one: |
| logicalChannelList:
allSizes: |
| semistaticTF_Information:
| channelCodingType:
turbo: |
rateMatchingAttribute: | 130
crc_Size: | crc16
transportChannelIdentity: | 14
ctch_Indicator: | false
| pich_Info:
| fdd:
channelisationCode256: | 2
pi_CountPerFrame: | e18
sttd_Indicator: | false
| cbs_DRX_Level1Information: Omit
| nonCriticalExtensions: Omit
| Outputs:
BITSTRING: |
[0] | 00 | 01 | 01 | 01 | 01 | 00 | 01 | 00
[8] | 00 | 11 | 11 | 10 | 00 | 00 | 00 | 00
[16] | 11 | 11 | 11 | 11 | 01 | 00 | 00 | 11
[24] | 11 | 11 | 11 | 11 | 11 | 11 | 11 | 01
[32] | 11 | 01 | 00 | 10 | 00 | 01 | 00 | 00
[40] | 11 | 11 | 00 | 00 | 00 | 10 | 10 | 01
[48] | 00 | 00 | 11 | 00 | 00 | 00 | 10 | 10
[56] | 10 | 10 | 01 | 01 | 01 | 01 | 10 | 00
[64] | 00 | 00 | 00 | 00 | 00 | 00 | 11 | 00
[72] | 11 | 00 | 01 | 01 | 10 | 11 | 01 | 01
[80] | 01 | 11 | 11 | 10 | 00 | 10 | 10 | 11
[88] | 10 | 10 | 00 | 00 | 11 | 11 | 11 | 10
[96] | 10 | 00 | 00 | 11 | 11 | 11 | 10 | 10
[104] | 00 | 00 | 11 | 11 | 11 | 10 | 10 | 00
[112] | 00 | 11 | 11 | 11 | 11 | 01 | 00 | 00
[120] | 00 | 00 | 00 | 00 | 00 | 00 | 00 | 11
[128] | 01 | 01 | 10 | 00 | 11 | 01 | 00 | 01
[136] | 00 | 00 | 11 | 11 | 11 | 01 | 00 | 11
[144] | 10 | 01 | 01 | 00 | 00 | 01 | 10 | 00
[152] | 01 | 00 | 00 | 11 | 00 | 10 | 10 | 00
[160] | 00 | 00 | 11 | 00 | 00 | 00 | 11 | 10
[168] | 00 | 00 | 01 | 00 | 00 | 00 | 01 | 01
[176] | 10 | 00 | 00 | 10 | 00 | 00 | 00 | 11
[184] | 10 | 00 | 00 | 00 | 00 | 10 | 00 | 10
[192] | 00 | 01 | 10 | 01 | 00 | 00 | 10 | 10
[200] | 01 | 10 | 01 | 00 | 00 | 10 | 10 | 00
[208] | 00 | 00 | 00 | 00 | 11 | 00 | 00 | 00
[216] | 01 | 00 | 01 | 00 | 01 | 01 | 11 | 00
[224] | 10 | 10 | 11 | 01 | 01 | 10 | 10 | 00
[232] | 00 | 00 | 00 | 00 | 01 | 11 | 10 | 00
[240] | 10 | 00 | 01 | 10 | 00 | 00 | 00 | 01
[248] | 01 | 10 | 11 | 01 | 10 | 11 | 01 | 10
[256] | 00 | 10 | 00 | 00 | 00 | 00 | 01 | 00
[264] | 00 | 11 | 00 | 00 | 10 | 00 | 10 | 01
[272] | 01 | 00 | 00 | 00 | 10 | 11 | 01 | 10
[280] | 10 | 00 | 00 | 00 | 01 | 00 | 00 |

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:08.640

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 22
bcch_ModificationTime: | Omit

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:08.650

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:08.650

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
noSegment: |

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA |  | RLC | @ 00:00:08.650

| Channel No: |  | 0 Name: BCCH

| Message Details:
| SIB repetition rate: 64
| SIB position: 44
| BCCH_BCH_Message:
| message:
| sfn_Prime: 0
| payload:
| noSegment: NULL
Layer 3 SDU: |
[0] | 00 | 00 |  |  |  |  |  |

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:08.650

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 18
bcch_ModificationTime: | Omit

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:08.670

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:08.670

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
| firstSegment:
sib_Type: | systemInformationBlockType5
seg_Count (SegCount): | 3
sib_Data_fixed: | 000101010100010000111110000000001111111101000011111111111111110111010010000100001111000000101001000011000000101010100101010110000000000000001100110001011011010101111110001010111010000011111110100000111111101000001111111010

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA |  | RLC | @ 00:00:08.670

| Channel No: |  | 0 Name: BCCH

| Message Details:
| SIB repetition rate: 64
| SIB position: 36
| BCCH_BCH_Message:
| message:
| sfn_Prime: 0
| payload:
| firstSegment:
| sib_Type: systemInformationBlockType5_SIB_Type [enum=5]
| seg_Count: 3
| sib_Data_fixed: 000101010100010000111110000000001111111101000011111111111111110111010010000100001111000000101001000011000000101010100101010110000000000000001100110001011011010101111110001010111010000011111110100000111111101000001111111010
Layer 3 SDU: |
[0] | 00 | 02 | 52 | 15 | 44 | 3E | 00 | FF
[8] | 43 | FF | FD | D2 | 10 | F0 | 29 | 0C
[16] | 0A | A5 | 58 | 00 | 0C | C5 | B5 | 7E
[24] | 2B | A0 | FE | 83 | FA | 0F | E8 |

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:08.670

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 19
bcch_ModificationTime: | Omit

#### MAC_DATA_REQ

RLC |  | MAC | @ 00:00:08.670

| Category: |  | Configuration
| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCCH
| CFN: |  | 108

| Message Details:
RLC PDU size (bits): | 184
RLC PDU (raw): |
[0] | 00 | 0E | 27 | 17 | 82 | 80 | 81 | 1B
[8] | 7A | 00 | 00 | 00 | 05 | B8 | C0 | 00
[16] | 80 | 12 | 10 | 23 | FF | FF | F8 |

#### MAC_DATA_REQ

RLC |  | MAC | @ 00:00:08.670

| Category: |  | Configuration
| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCCH
| CFN: |  | 108

| Message Details:
RLC PDU size (bits): | 168
RLC PDU (raw): |
[0] | 00 | 0E | 27 | 17 | 82 | 80 | 81 | 22
[8] | F0 | 00 | 00 | 00 | 0B | 71 | 80 | 01
[16] | 00 | 24 | 00 | 47 | 70 |  |  |

#### MAC_DATA_REQ

RLC |  | MAC | @ 00:00:08.670

| Category: |  | Configuration
| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCCH
| CFN: |  | 108

| Message Details:
RLC PDU size (bits): | 16
RLC PDU (raw): |
[0] | 00 | 00 |  |  |  |  |  |

#### PHY_DATA_REQ

MAC |  | PHY | @ 00:00:08.670

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCH
| CFN: |  | 108

| Message Details:
SIB repetition period: | 64
SIB position: | 14
SIB size: | 246
SIB (raw): |
[0] | 00 | 0E | 27 | 17 | 82 | 80 | 81 | 1B
[8] | 7A | 00 | 00 | 00 | 05 | B8 | C0 | 00
[16] | 80 | 12 | 10 | 23 | FF | FF | F8 | 4C
[24] | 42 | 60 | 00 | 02 | 00 | 00 | 00 | 00
| SIB (decoded):
| TB 0:
MAC SDU (246 bits): |
[0] | 00 | 0E | 27 | 17 | 82 | 80 | 81 | 1B
[8] | 7A | 00 | 00 | 00 | 05 | B8 | C0 | 00
[16] | 80 | 12 | 10 | 23 | FF | FF | F8 | 4C
[24] | 42 | 60 | 00 | 02 | 00 | 00 | 00 |

#### MAC_DATA_REQ

RLC |  | MAC | @ 00:00:08.680

| Category: |  | Configuration
| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCCH
| CFN: |  | 109

| Message Details:
RLC PDU size (bits): | 248
RLC PDU (raw): |
[0] | 00 | 02 | 52 | 15 | 44 | 3E | 00 | FF
[8] | 43 | FF | FD | D2 | 10 | F0 | 29 | 0C
[16] | 0A | A5 | 58 | 00 | 0C | C5 | B5 | 7E
[24] | 2B | A0 | FE | 83 | FA | 0F | E8 |

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:08.690

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:08.690

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
| subsequentSegment:
sib_Type: | systemInformationBlockType5
segmentIndex: | 1
sib_Data_fixed: | 000011111111010000000000000000001101011000110100010000111111010011100101000001100001000011001010000000110000001110000001000000010110000010000000111000000000100010000110010000101001100100001010000000000011000000010001000101

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA |  | RLC | @ 00:00:08.690

| Channel No: |  | 0 Name: BCCH

| Message Details:
| SIB repetition rate: 64
| SIB position: 38
| BCCH_BCH_Message:
| message:
| sfn_Prime: 0
| payload:
| subsequentSegment:
| sib_Type: systemInformationBlockType5_SIB_Type [enum=5]
| segmentIndex: 1
| sib_Data_fixed: 000011111111010000000000000000001101011000110100010000111111010011100101000001100001000011001010000000110000001110000001000000010110000010000000111000000000100010000110010000101001100100001010000000000011000000010001000101
Layer 3 SDU: |
[0] | 00 | 04 | 50 | 0F | F4 | 00 | 00 | D6
[8] | 34 | 43 | F4 | E5 | 06 | 10 | CA | 03
[16] | 03 | 81 | 01 | 60 | 80 | E0 | 08 | 86
[24] | 42 | 99 | 0A | 00 | 30 | 11 | 14 |

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:08.690

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 21
bcch_ModificationTime: | Omit

#### PHY_DATA_REQ

MAC |  | PHY | @ 00:00:08.690

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCH
| CFN: |  | 110

| Message Details:
SIB repetition period: | 64
SIB position: | 62
SIB size: | 246
SIB (raw): |
[0] | 00 | 0E | 27 | 17 | 82 | 80 | 81 | 22
[8] | F0 | 00 | 00 | 00 | 0B | 71 | 80 | 01
[16] | 00 | 24 | 00 | 47 | 70 | FF | F8 | 4C
[24] | 42 | 60 | 00 | 02 | 00 | 00 | 00 | 00
| SIB (decoded):
| TB 0:
MAC SDU (246 bits): |
[0] | 00 | 0E | 27 | 17 | 82 | 80 | 81 | 22
[8] | F0 | 00 | 00 | 00 | 0B | 71 | 80 | 01
[16] | 00 | 24 | 00 | 47 | 70 | FF | F8 | 4C
[24] | 42 | 60 | 00 | 02 | 00 | 00 | 00 |

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:08.700

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:08.700

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
| lastSegmentShort:
sib_Type: | systemInformationBlockType5
segmentIndex: | 2
sib_Data_variable: | 1100101011010110100000000000011110001000011000000001011011011011011000100000000001000011000010001001010000001011011010000000010000

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA |  | RLC | @ 00:00:08.700

| Channel No: |  | 0 Name: BCCH

| Message Details:
| SIB repetition rate: 64
| SIB position: 42
| BCCH_BCH_Message:
| message:
| sfn_Prime: 0
| payload:
| lastSegmentShort:
| sib_Type: systemInformationBlockType5_SIB_Type [enum=5]
| segmentIndex: 2
| sib_Data_variable: 1100101011010110100000000000011110001000011000000001011011011011011000100000000001000011000010001001010000001011011010000000010000
Layer 3 SDU: |
[0] | 00 | 06 | 51 | 81 | CA | D6 | 80 | 07
[8] | 88 | 60 | 16 | DB | 62 | 00 | 43 | 08
[16] | 94 | 0B | 68 | 04 | 00 |  |  |

#### o_SIB_PER_Encoding

RRC |  | RRC | @ 00:00:08.700

| Category: |  | TSO

| Message Details:
| Inputs:
| SIB:
| sIB6: (SysInfoType6)
pich_PowerOffset: | -5
| modeSpecificInfo:
| fdd:
aich_PowerOffset: | -5
dummy (CSICH_PowerOffset): | Omit
| primaryCCPCH_Info: Omit
| prach_SystemInformationList: Omit
| sCCPCH_SystemInformationList: Omit
| cbs_DRX_Level1Information: Omit
| nonCriticalExtensions: Omit
| Outputs:
BITSTRING: |
[0] | 00 | 00 | 00 | 10 | 10 | 01 | 00 | 01

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:08.700

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 2
bcch_ModificationTime: | Omit

#### MAC_DATA_REQ

RLC |  | MAC | @ 00:00:08.710

| Category: |  | Configuration
| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCCH
| CFN: |  | 112

| Message Details:
RLC PDU size (bits): | 248
RLC PDU (raw): |
[0] | 00 | 04 | 50 | 0F | F4 | 00 | 00 | D6
[8] | 34 | 43 | F4 | E5 | 06 | 10 | CA | 03
[16] | 03 | 81 | 01 | 60 | 80 | E0 | 08 | 86
[24] | 42 | 99 | 0A | 00 | 30 | 11 | 14 |

#### MAC_DATA_REQ

RLC |  | MAC | @ 00:00:08.710

| Category: |  | Configuration
| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCCH
| CFN: |  | 112

| Message Details:
RLC PDU size (bits): | 168
RLC PDU (raw): |
[0] | 00 | 06 | 51 | 81 | CA | D6 | 80 | 07
[8] | 88 | 60 | 16 | DB | 62 | 00 | 43 | 08
[16] | 94 | 0B | 68 | 04 | 00 |  |  |

#### PHY_DATA_REQ

MAC |  | PHY | @ 00:00:08.710

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCH
| CFN: |  | 112

| Message Details:
SIB repetition period: | 64
SIB position: | 44
SIB size: | 246
SIB (raw): |
[0] | 00 | 00 | 27 | 17 | 82 | 80 | 81 | 22
[8] | F0 | 00 | 00 | 00 | 0B | 71 | 80 | 01
[16] | 00 | 24 | 00 | 47 | 70 | FF | F8 | 4C
[24] | 42 | 60 | 00 | 02 | 00 | 00 | 00 | 00
| SIB (decoded):
| TB 0:
MAC SDU (246 bits): |
[0] | 00 | 00 | 27 | 17 | 82 | 80 | 81 | 22
[8] | F0 | 00 | 00 | 00 | 0B | 71 | 80 | 01
[16] | 00 | 24 | 00 | 47 | 70 | FF | F8 | 4C
[24] | 42 | 60 | 00 | 02 | 00 | 00 | 00 |

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:08.720

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:08.720

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
| completeSIB_List:
| CompleteSIBshort:
sib_Type: | systemInformationBlockType6
sib_Data_variable: | 0000001010010001

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA |  | RLC | @ 00:00:08.720

| Channel No: |  | 0 Name: BCCH

| Message Details:
| SIB repetition rate: 64
| SIB position: 4
| BCCH_BCH_Message:
| message:
| sfn_Prime: 0
| payload:
| completeSIB_List:
| CompleteSIB_List.element:
| sib_Type: systemInformationBlockType6_SIB_Type [enum=6]
| sib_Data_variable: 0000001010010001
Layer 3 SDU: |
[0] | 00 | 0E | 06 | 0F | 02 | 91 |  |

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:08.720

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 3
bcch_ModificationTime: | Omit

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:08.730

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:08.730

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
noSegment: |

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA |  | RLC | @ 00:00:08.730

| Channel No: |  | 0 Name: BCCH

| Message Details:
| SIB repetition rate: 64
| SIB position: 6
| BCCH_BCH_Message:
| message:
| sfn_Prime: 0
| payload:
| noSegment: NULL
Layer 3 SDU: |
[0] | 00 | 00 |  |  |  |  |  |

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:08.730

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 5
bcch_ModificationTime: | Omit

#### PHY_DATA_REQ

MAC |  | PHY | @ 00:00:08.730

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCH
| CFN: |  | 114

| Message Details:
SIB repetition period: | 64
SIB position: | 36
SIB size: | 246
SIB (raw): |
[0] | 00 | 02 | 52 | 15 | 44 | 3E | 00 | FF
[8] | 43 | FF | FD | D2 | 10 | F0 | 29 | 0C
[16] | 0A | A5 | 58 | 00 | 0C | C5 | B5 | 7E
[24] | 2B | A0 | FE | 83 | FA | 0F | E8 | 00
| SIB (decoded):
| TB 0:
MAC SDU (246 bits): |
[0] | 00 | 02 | 52 | 15 | 44 | 3E | 00 | FF
[8] | 43 | FF | FD | D2 | 10 | F0 | 29 | 0C
[16] | 0A | A5 | 58 | 00 | 0C | C5 | B5 | 7E
[24] | 2B | A0 | FE | 83 | FA | 0F | E8 |

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:08.750

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:08.750

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
noSegment: |

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA |  | RLC | @ 00:00:08.750

| Channel No: |  | 0 Name: BCCH

| Message Details:
| SIB repetition rate: 64
| SIB position: 10
| BCCH_BCH_Message:
| message:
| sfn_Prime: 0
| payload:
| noSegment: NULL
Layer 3 SDU: |
[0] | 00 | 00 |  |  |  |  |  |

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:08.750

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 6
bcch_ModificationTime: | Omit

#### PHY_DATA_REQ

MAC |  | PHY | @ 00:00:08.750

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCH
| CFN: |  | 116

| Message Details:
SIB repetition period: | 64
SIB position: | 38
SIB size: | 246
SIB (raw): |
[0] | 00 | 04 | 50 | 0F | F4 | 00 | 00 | D6
[8] | 34 | 43 | F4 | E5 | 06 | 10 | CA | 03
[16] | 03 | 81 | 01 | 60 | 80 | E0 | 08 | 86
[24] | 42 | 99 | 0A | 00 | 30 | 11 | 14 | 00
| SIB (decoded):
| TB 0:
MAC SDU (246 bits): |
[0] | 00 | 04 | 50 | 0F | F4 | 00 | 00 | D6
[8] | 34 | 43 | F4 | E5 | 06 | 10 | CA | 03
[16] | 03 | 81 | 01 | 60 | 80 | E0 | 08 | 86
[24] | 42 | 99 | 0A | 00 | 30 | 11 | 14 |

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:08.760

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:08.760

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
noSegment: |

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA |  | RLC | @ 00:00:08.760

| Channel No: |  | 0 Name: BCCH

| Message Details:
| SIB repetition rate: 64
| SIB position: 12
| BCCH_BCH_Message:
| message:
| sfn_Prime: 0
| payload:
| noSegment: NULL
Layer 3 SDU: |
[0] | 00 | 00 |  |  |  |  |  |

#### o_SIB_PER_Encoding

RRC |  | RRC | @ 00:00:08.760

| Category: |  | TSO

| Message Details:
| Inputs:
| SIB:
| sIB7: (SysInfoType7)
| modeSpecificInfo:
| fdd:
ul_Interference: | -100
| prach_Information_SIB5_List: (DynamicPersistenceLevelList)
DynamicPersistenceLevel: | 2
| prach_Information_SIB6_List: (DynamicPersistenceLevelList)
DynamicPersistenceLevel: | 2
expirationTimeFactor: | Omit
| nonCriticalExtensions: Omit
| Outputs:
BITSTRING: |
[0] | 10 | 00 | 00 | 10 | 10 | 00 | 00 | 00
[8] | 10 | 00 | 00 | 01 |  |  |  |

#### PHY_DATA_REQ

MAC |  | PHY | @ 00:00:08.770

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCH
| CFN: |  | 118

| Message Details:
SIB repetition period: | 64
SIB position: | 42
SIB size: | 246
SIB (raw): |
[0] | 00 | 06 | 51 | 81 | CA | D6 | 80 | 07
[8] | 88 | 60 | 16 | DB | 62 | 00 | 43 | 08
[16] | 94 | 0B | 68 | 04 | 00 | E0 | 08 | 86
[24] | 42 | 99 | 0A | 00 | 30 | 11 | 14 | 00
| SIB (decoded):
| TB 0:
MAC SDU (246 bits): |
[0] | 00 | 06 | 51 | 81 | CA | D6 | 80 | 07
[8] | 88 | 60 | 16 | DB | 62 | 00 | 43 | 08
[16] | 94 | 0B | 68 | 04 | 00 | E0 | 08 | 86
[24] | 42 | 99 | 0A | 00 | 30 | 11 | 14 |

#### o_SIB_PER_Encoding

RRC |  | RRC | @ 00:00:08.780

| Category: |  | TSO

| Message Details:
| Inputs:
| SIB:
| sIB12: (SysInfoType12)
| fach_MeasurementOccasionInfo: Omit
| measurementControlSysInfo:
| use_of_HCS:
| hcs_not_used:
| cellSelectQualityMeasure:
| cpich_RSCP:
| intraFreqMeasurementSysInfo: (IntraFreqMeasurementSysInfo_RSCP)
intraFreqMeasurementID (MeasurementIdentity): | Omit
| intraFreqCellInfoSI_List: (IntraFreqCellInfoSI_List_RSCP)
| removedIntraFreqCellList: Omit
| newIntraFreqCellList: (NewIntraFreqCellSI_List_RSCP)
| NewIntraFreqCellSI_RSCP:
intraFreqCellID: | 1
| cellInfo: (CellInfoSI_RSCP)
cellIndividualOffset: | Omit
| referenceTimeDifferenceToCell: Omit
| modeSpecificInfo:
| fdd:
| primaryCPICH_Info:
primaryScramblingCode: | 150
primaryCPICH_TX_Power: | Omit
readSFN_Indicator: | true
tx_DiversityIndicator: | false
| cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP)
q_OffsetS_N: | 0
maxAllowedUL_TX_Power: | 21
| modeSpecificInfo:
| fdd:
q_QualMin: | -16
q_RxlevMin: | -58
| NewIntraFreqCellSI_RSCP:
intraFreqCellID: | 2
| cellInfo: (CellInfoSI_RSCP)
cellIndividualOffset: | Omit
| referenceTimeDifferenceToCell: Omit
| modeSpecificInfo:
| fdd:
| primaryCPICH_Info:
primaryScramblingCode: | 200
primaryCPICH_TX_Power: | Omit
readSFN_Indicator: | true
tx_DiversityIndicator: | false
| cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP)
q_OffsetS_N: | 0
maxAllowedUL_TX_Power: | 21
| modeSpecificInfo:
| fdd:
q_QualMin: | -16
q_RxlevMin: | -58
| intraFreqMeasQuantity:
filterCoefficient: | Omit
| modeSpecificInfo:
| fdd:
intraFreqMeasQuantity_FDD: | cpich_RSCP
| intraFreqReportingQuantityForRACH: Omit
maxReportedCellsOnRACH: | Omit
| reportingInfoForCellDCH:
| intraFreqReportingQuantity:
| activeSetReportingQuantities: (CellReportingQuantities)
dummy (SFN_SFN_OTD_Type): | noReport
cellIdentity_reportingIndicator: | true
cellSynchronisationInfoReportingIndicator: | false
| modeSpecificInfo:
| fdd:
cpich_Ec_N0_reportingIndicator: | false
cpich_RSCP_reportingIndicator: | true
pathloss_reportingIndicator: | false
| monitoredSetReportingQuantities: (CellReportingQuantities)
dummy (SFN_SFN_OTD_Type): | noReport
cellIdentity_reportingIndicator: | true
cellSynchronisationInfoReportingIndicator: | true
| modeSpecificInfo:
| fdd:
cpich_Ec_N0_reportingIndicator: | false
cpich_RSCP_reportingIndicator: | true
pathloss_reportingIndicator: | false
| detectedSetReportingQuantities: (CellReportingQuantities) Omit
| measurementReportingMode:
measurementReportTransferMode (TransferMode): | acknowledgedModeRLC
periodicalOrEventTrigger: | eventTrigger
| reportCriteria: (CellDCH_ReportCriteria)
| intraFreqReportingCriteria:
| eventCriteriaList: (IntraFreqEventCriteriaList)
| IntraFreqEventCriteria:
| event: (IntraFreqEvent)
| e1a: (Event1a)
triggeringCondition (TriggeringCondition2): | monitoredSetCellsOnly
reportingRange: | 5
| forbiddenAffectCellList: Omit
w: | 1
reportDeactivationThreshold: | t2
reportingAmount: | ra4
reportingInterval: | noPeriodicalreporting
hysteresis: | 0
timeToTrigger: | ttt640
| reportingCellStatus:
withinActiveAndOrMonitoredUsedFreq (MaxNumberOfReportingCellsType1): | e3
| IntraFreqEventCriteria:
| event: (IntraFreqEvent)
| e1b: (Event1b)
triggeringCondition (TriggeringCondition1): | activeSetCellsOnly
reportingRange: | 5
| forbiddenAffectCellList: Omit
w: | 1
hysteresis: | 0
timeToTrigger: | ttt640
| reportingCellStatus:
withinActiveAndOrMonitoredUsedFreq (MaxNumberOfReportingCellsType1): | e3
| IntraFreqEventCriteria:
| event: (IntraFreqEvent)
| e1c: (Event1c)
replacementActivationThreshold: | t3
reportingAmount: | ra4
reportingInterval: | ri4
hysteresis: | 0
timeToTrigger: | ttt640
| reportingCellStatus:
withinActiveAndOrMonitoredUsedFreq (MaxNumberOfReportingCellsType1): | e3
| interFreqMeasurementSysInfo: (InterFreqMeasurementSysInfo_RSCP)
| interFreqCellInfoSI_List: (InterFreqCellInfoSI_List_RSCP)
| removedInterFreqCellList: Omit
| newInterFreqCellList: (NewInterFreqCellSI_List_RSCP)
| NewInterFreqCellSI_RSCP:
interFreqCellID: | 3
| frequencyInfo:
| modeSpecificInfo:
| fdd: (FrequencyInfoFDD)
uarfcn_UL (UARFCN): | 9663
uarfcn_DL (UARFCN): | 10613
| cellInfo: (CellInfoSI_RSCP)
cellIndividualOffset: | Omit
| referenceTimeDifferenceToCell: Omit
| modeSpecificInfo:
| fdd:
| primaryCPICH_Info:
primaryScramblingCode: | 200
primaryCPICH_TX_Power: | Omit
readSFN_Indicator: | true
tx_DiversityIndicator: | false
| cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP)
q_OffsetS_N: | 0
maxAllowedUL_TX_Power: | 21
| modeSpecificInfo:
| fdd:
q_QualMin: | -16
q_RxlevMin: | -58
| NewInterFreqCellSI_RSCP:
interFreqCellID: | 4
| frequencyInfo: Omit
| cellInfo: (CellInfoSI_RSCP)
cellIndividualOffset: | Omit
| referenceTimeDifferenceToCell: Omit
| modeSpecificInfo:
| fdd:
| primaryCPICH_Info:
primaryScramblingCode: | 300
primaryCPICH_TX_Power: | Omit
readSFN_Indicator: | true
tx_DiversityIndicator: | false
| cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP)
q_OffsetS_N: | 0
maxAllowedUL_TX_Power: | 21
| modeSpecificInfo:
| fdd:
q_QualMin: | -16
q_RxlevMin: | -58
| NewInterFreqCellSI_RSCP:
interFreqCellID: | 5
| frequencyInfo: Omit
| cellInfo: (CellInfoSI_RSCP)
cellIndividualOffset: | Omit
| referenceTimeDifferenceToCell: Omit
| modeSpecificInfo:
| fdd:
| primaryCPICH_Info:
primaryScramblingCode: | 350
primaryCPICH_TX_Power: | Omit
readSFN_Indicator: | true
tx_DiversityIndicator: | false
| cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP)
q_OffsetS_N: | 0
maxAllowedUL_TX_Power: | 21
| modeSpecificInfo:
| fdd:
q_QualMin: | -16
q_RxlevMin: | -58
| NewInterFreqCellSI_RSCP:
interFreqCellID: | 4
| frequencyInfo:
| modeSpecificInfo:
| fdd: (FrequencyInfoFDD)
uarfcn_UL (UARFCN): | 9713
uarfcn_DL (UARFCN): | 10663
| cellInfo: (CellInfoSI_RSCP)
cellIndividualOffset: | Omit
| referenceTimeDifferenceToCell: Omit
| modeSpecificInfo:
| fdd:
| primaryCPICH_Info:
primaryScramblingCode: | 150
primaryCPICH_TX_Power: | Omit
readSFN_Indicator: | true
tx_DiversityIndicator: | false
| cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP)
q_OffsetS_N: | 0
maxAllowedUL_TX_Power: | 21
| modeSpecificInfo:
| fdd:
q_QualMin: | -16
q_RxlevMin: | -58
| NewInterFreqCellSI_RSCP:
interFreqCellID: | 7
| frequencyInfo: Omit
| cellInfo: (CellInfoSI_RSCP)
cellIndividualOffset: | Omit
| referenceTimeDifferenceToCell: Omit
| modeSpecificInfo:
| fdd:
| primaryCPICH_Info:
primaryScramblingCode: | 450
primaryCPICH_TX_Power: | Omit
readSFN_Indicator: | true
tx_DiversityIndicator: | false
| cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP)
q_OffsetS_N: | 0
maxAllowedUL_TX_Power: | 21
| modeSpecificInfo:
| fdd:
q_QualMin: | -16
q_RxlevMin: | -58
| interRATMeasurementSysInfo: (InterRATMeasurementSysInfo_B) Omit
| trafficVolumeMeasSysInfo: Omit
| dummy: (UE_InternalMeasurementSysInfo) Omit
| nonCriticalExtensions: Omit
| Outputs:
BITSTRING: |
[0] | 00 | 00 | 00 | 01 | 10 | 11 | 00 | 10
[8] | 00 | 00 | 11 | 00 | 00 | 10 | 01 | 01
[16] | 00 | 10 | 01 | 01 | 10 | 10 | 01 | 10
[24] | 00 | 11 | 10 | 01 | 10 | 10 | 00 | 00
[32] | 00 | 00 | 10 | 00 | 10 | 00 | 10 | 10
[40] | 01 | 10 | 01 | 00 | 01 | 00 | 11 | 00
[48] | 01 | 11 | 00 | 11 | 01 | 00 | 00 | 00
[56] | 00 | 00 | 00 | 10 | 00 | 10 | 00 | 10
[64] | 00 | 11 | 00 | 10 | 01 | 01 | 01 | 01
[72] | 00 | 00 | 00 | 01 | 00 | 10 | 10 | 00
[80] | 01 | 01 | 00 | 10 | 00 | 00 | 00 | 01
[88] | 10 | 00 | 01 | 00 | 10 | 10 | 00 | 10
[96] | 00 | 00 | 10 | 10 | 00 | 01 | 00 | 00
[104] | 11 | 00 | 00 | 10 | 01 | 01 | 00 | 10
[112] | 01 | 10 | 10 | 10 | 10 | 00 | 01 | 10
[120] | 00 | 01 | 00 | 10 | 10 | 10 | 01 | 00
[128] | 11 | 00 | 01 | 10 | 11 | 00 | 10 | 11
[136] | 01 | 11 | 11 | 11 | 01 | 00 | 10 | 11
[144] | 10 | 10 | 10 | 01 | 01 | 00 | 11 | 00
[152] | 10 | 00 | 10 | 01 | 10 | 00 | 11 | 10
[160] | 01 | 10 | 10 | 00 | 00 | 00 | 00 | 10
[168] | 00 | 10 | 00 | 01 | 01 | 01 | 00 | 10
[176] | 11 | 00 | 10 | 01 | 10 | 00 | 11 | 10
[184] | 01 | 10 | 10 | 00 | 00 | 00 | 00 | 10
[192] | 00 | 10 | 10 | 01 | 01 | 01 | 01 | 01
[200] | 11 | 10 | 10 | 01 | 10 | 00 | 11 | 10
[208] | 01 | 10 | 10 | 00 | 00 | 00 | 00 | 11
[216] | 00 | 10 | 00 | 11 | 00 | 10 | 11 | 11
[224] | 10 | 00 | 11 | 01 | 00 | 11 | 01 | 00
[232] | 11 | 10 | 01 | 01 | 00 | 10 | 01 | 01
[240] | 10 | 10 | 01 | 10 | 00 | 11 | 10 | 01
[248] | 10 | 10 | 00 | 00 | 00 | 00 | 10 | 00
[256] | 11 | 10 | 01 | 01 | 01 | 11 | 00 | 00
[264] | 10 | 10 | 01 | 10 | 00 | 11 | 10 | 01
[272] | 10 | 10 | 00 | 00 | 00 | 00 |  |

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:08.780

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 15
bcch_ModificationTime: | Omit

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:08.790

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:08.790

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
| completeSIB_List:
| CompleteSIBshort:
sib_Type: | systemInformationBlockType7
sib_Data_variable: | 100000101000000010000001

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA |  | RLC | @ 00:00:08.790

| Channel No: |  | 0 Name: BCCH

| Message Details:
| SIB repetition rate: 64
| SIB position: 30
| BCCH_BCH_Message:
| message:
| sfn_Prime: 0
| payload:
| completeSIB_List:
| CompleteSIB_List.element:
| sib_Type: systemInformationBlockType7_SIB_Type [enum=7]
| sib_Data_variable: 100000101000000010000001
Layer 3 SDU: |
[0] | 00 | 0E | 07 | 17 | 82 | 80 | 81 |

#### o_SIB_PER_Encoding

RRC |  | RRC | @ 00:00:08.790

| Category: |  | TSO

| Message Details:
| Inputs:
| SIB:
| sIB3: (SysInfoType3)
sib4indicator: | true
cellIdentity: | 0000000000000000000000000000
| cellSelectReselectInfo: (CellSelectReselectInfoSIB_3_4)
| mappingInfo: Omit
| cellSelectQualityMeasure:
cpich_RSCP: |
| modeSpecificInfo:
| fdd:
s_Intrasearch (S_SearchQual): | 8
s_Intersearch (S_SearchQual): | 8
s_SearchHCS (S_SearchRXLEV): | Omit
| rat_List: (RAT_FDD_InfoList)
| RAT_FDD_Info:
rat_Identifier: | gsm
s_SearchRAT (S_SearchQual): | -16
s_HCS_RAT (S_SearchRXLEV): | Omit
s_Limit_SearchRAT (S_SearchQual): | 0
q_QualMin: | -24
q_RxlevMin: | -40
q_Hyst_l_S (Q_Hyst_S): | 2
t_Reselection_S: | 0
| hcs_ServingCellInformation: Omit
maxAllowedUL_TX_Power: | 21
| cellAccessRestriction:
| cellBarred:
notBarred: |
cellReservedForOperatorUse (ReservedIndicator): | notReserved
cellReservationExtension (ReservedIndicator): | notReserved
| accessClassBarredList:
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
| nonCriticalExtensions: Omit
| Outputs:
BITSTRING: |
[0] | 01 | 00 | 00 | 00 | 00 | 00 | 00 | 00
[8] | 00 | 00 | 00 | 00 | 00 | 00 | 00 | 00
[16] | 10 | 11 | 01 | 11 | 00 | 01 | 10 | 00
[24] | 00 | 00 | 00 | 00 | 00 | 01 | 00 | 00
[32] | 00 | 00 | 00 | 10 | 01 | 00 | 00 | 10
[40] | 00 | 00 | 01 | 00 | 01 | 11 | 11 | 11
[48] | 11 | 11 | 11 | 11 | 11 | 11 | 11 | 11

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:08.790

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 7
bcch_ModificationTime: | Omit

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:08.810

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:08.810

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
| completeSIB_List:
| CompleteSIBshort:
sib_Type: | systemInformationBlockType7
sib_Data_variable: | 100000101000000010000001
| CompleteSIBshort:
sib_Type: | systemInformationBlockType3
sib_Data_variable: | 0100000000000000000000000000000010110111000110000000000000010000000000100100001000000100011111111111111111111111

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA |  | RLC | @ 00:00:08.810

| Channel No: |  | 0 Name: BCCH

| Message Details:
| SIB repetition rate: 64
| SIB position: 14
| BCCH_BCH_Message:
| message:
| sfn_Prime: 0
| payload:
| completeSIB_List:
| CompleteSIB_List.element:
| sib_Type: systemInformationBlockType7_SIB_Type [enum=7]
| sib_Data_variable: 100000101000000010000001
| CompleteSIB_List.element:
| sib_Type: systemInformationBlockType3_SIB_Type [enum=3]
| sib_Data_variable: 0100000000000000000000000000000010110111000110000000000000010000000000100100001000000100011111111111111111111111
Layer 3 SDU: |
[0] | 00 | 0E | 27 | 17 | 82 | 80 | 81 | 1B
[8] | 7A | 00 | 00 | 00 | 05 | B8 | C0 | 00
[16] | 80 | 12 | 10 | 23 | FF | FF | F8 |

#### o_SIB_PER_Encoding

RRC |  | RRC | @ 00:00:08.810

| Category: |  | TSO

| Message Details:
| Inputs:
| SIB:
| sIB18: (SysInfoType18)
| idleModePLMNIdentities: (PLMNIdentitiesOfNeighbourCells)
| plmnsOfIntraFreqCellsList: Omit
| plmnsOfInterFreqCellsList:
| :
| plmn_Identity:
| mcc:
Digit: | 0
Digit: | 0
Digit: | 2
| mnc:
Digit: | 1
Digit: | 1
| :
| plmn_Identity:
| mcc:
Digit: | 0
Digit: | 0
Digit: | 2
| mnc:
Digit: | 1
Digit: | 1
| :
| plmn_Identity:
| mcc:
Digit: | 0
Digit: | 0
Digit: | 2
| mnc:
Digit: | 1
Digit: | 1
| :
| plmn_Identity:
| mcc:
Digit: | 0
Digit: | 0
Digit: | 4
| mnc:
Digit: | 2
Digit: | 1
| plmnsOfInterRATCellsList: Omit
| connectedModePLMNIdentities: (PLMNIdentitiesOfNeighbourCells) Omit
| nonCriticalExtensions: Omit
| Outputs:
BITSTRING: |
[0] | 10 | 00 | 10 | 00 | 01 | 11 | 00 | 00
[8] | 00 | 00 | 00 | 10 | 00 | 00 | 10 | 00
[16] | 11 | 00 | 00 | 00 | 00 | 00 | 10 | 00
[24] | 00 | 10 | 00 | 11 | 00 | 00 | 00 | 00
[32] | 00 | 10 | 00 | 00 | 10 | 00 | 11 | 00
[40] | 00 | 00 | 00 | 01 | 00 | 00 | 01 | 00
[48] | 00 | 1 |  |  |  |  |  |

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:08.810

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 23
bcch_ModificationTime: | Omit

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:08.830

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:08.830

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
| completeSIB_List:
| CompleteSIBshort:
sib_Type: | systemInformationBlockType7
sib_Data_variable: | 100000101000000010000001
| CompleteSIBshort:
sib_Type: | systemInformationBlockType18
sib_Data_variable: | 100010000111000000000010000010001100000000001000001000110000000000100000100011000000000100000100001

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA |  | RLC | @ 00:00:08.830

| Channel No: |  | 0 Name: BCCH

| Message Details:
| SIB repetition rate: 64
| SIB position: 46
| BCCH_BCH_Message:
| message:
| sfn_Prime: 0
| payload:
| completeSIB_List:
| CompleteSIB_List.element:
| sib_Type: systemInformationBlockType7_SIB_Type [enum=7]
| sib_Data_variable: 100000101000000010000001
| CompleteSIB_List.element:
| sib_Type: systemInformationBlockType18_SIB_Type [enum=26]
| sib_Data_variable: 100010000111000000000010000010001100000000001000001000110000000000100000100011000000000100000100001
Layer 3 SDU: |
[0] | 00 | 0E | 27 | 17 | 82 | 80 | 81 | D3
[8] | 14 | 43 | 80 | 10 | 46 | 00 | 41 | 18
[16] | 01 | 04 | 60 | 08 | 21 |  |  |

#### o_SIB_PER_Encoding

RRC |  | RRC | @ 00:00:08.830

| Category: |  | TSO

| Message Details:
| Inputs:
| SIB:
| sIB4: (SysInfoType4)
cellIdentity: | 0000000000000000000000000000
| cellSelectReselectInfo: (CellSelectReselectInfoSIB_3_4)
| mappingInfo: Omit
| cellSelectQualityMeasure:
cpich_RSCP: |
| modeSpecificInfo:
| fdd:
s_Intrasearch (S_SearchQual): | 8
s_Intersearch (S_SearchQual): | 8
s_SearchHCS (S_SearchRXLEV): | Omit
| rat_List: (RAT_FDD_InfoList)
| RAT_FDD_Info:
rat_Identifier: | gsm
s_SearchRAT (S_SearchQual): | -16
s_HCS_RAT (S_SearchRXLEV): | Omit
s_Limit_SearchRAT (S_SearchQual): | 0
q_QualMin: | -24
q_RxlevMin: | -40
q_Hyst_l_S (Q_Hyst_S): | 0
t_Reselection_S: | 0
| hcs_ServingCellInformation: Omit
maxAllowedUL_TX_Power: | 21
| cellAccessRestriction:
| cellBarred:
notBarred: |
cellReservedForOperatorUse (ReservedIndicator): | notReserved
cellReservationExtension (ReservedIndicator): | notReserved
| accessClassBarredList: Omit
| nonCriticalExtensions: Omit
| Outputs:
BITSTRING: |
[0] | 00 | 00 | 00 | 00 | 00 | 00 | 00 | 00
[8] | 00 | 00 | 00 | 00 | 00 | 00 | 00 | 01
[16] | 01 | 10 | 11 | 10 | 00 | 11 | 00 | 00
[24] | 00 | 00 | 00 | 00 | 00 | 10 | 00 | 00
[32] | 00 | 00 | 01 | 00 | 10 | 00 | 00 | 00
[40] | 00 | 00 | 10 | 00 | 11 | 10 | 11 | 1

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:08.830

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 31
bcch_ModificationTime: | Omit

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:08.840

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:08.840

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
| completeSIB_List:
| CompleteSIBshort:
sib_Type: | systemInformationBlockType7
sib_Data_variable: | 100000101000000010000001
| CompleteSIBshort:
sib_Type: | systemInformationBlockType4
sib_Data_variable: | 00000000000000000000000000000001011011100011000000000000001000000000010010000000000010001110111

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA |  | RLC | @ 00:00:08.840

| Channel No: |  | 0 Name: BCCH

| Message Details:
| SIB repetition rate: 64
| SIB position: 62
| BCCH_BCH_Message:
| message:
| sfn_Prime: 0
| payload:
| completeSIB_List:
| CompleteSIB_List.element:
| sib_Type: systemInformationBlockType7_SIB_Type [enum=7]
| sib_Data_variable: 100000101000000010000001
| CompleteSIB_List.element:
| sib_Type: systemInformationBlockType4_SIB_Type [enum=4]
| sib_Data_variable: 00000000000000000000000000000001011011100011000000000000001000000000010010000000000010001110111
Layer 3 SDU: |
[0] | 00 | 0E | 27 | 17 | 82 | 80 | 81 | 22
[8] | F0 | 00 | 00 | 00 | 0B | 71 | 80 | 01
[16] | 00 | 24 | 00 | 47 | 70 |  |  |

#### o_SIB_PER_Encoding

RRC |  | RRC | @ 00:00:08.860

| Category: |  | TSO

| Message Details:
| Inputs:
| SIB:
| sIB11: (SysInfoType11)
sib12indicator: | true
| fach_MeasurementOccasionInfo: Omit
| measurementControlSysInfo:
| use_of_HCS:
| hcs_not_used:
| cellSelectQualityMeasure:
| cpich_RSCP:
| intraFreqMeasurementSysInfo: (IntraFreqMeasurementSysInfo_RSCP)
intraFreqMeasurementID (MeasurementIdentity): | Omit
| intraFreqCellInfoSI_List: (IntraFreqCellInfoSI_List_RSCP)
| removedIntraFreqCellList: Omit
| newIntraFreqCellList: (NewIntraFreqCellSI_List_RSCP)
| NewIntraFreqCellSI_RSCP:
intraFreqCellID: | 0
| cellInfo: (CellInfoSI_RSCP)
cellIndividualOffset: | Omit
| referenceTimeDifferenceToCell: Omit
| modeSpecificInfo:
| fdd:
| primaryCPICH_Info:
primaryScramblingCode: | 100
primaryCPICH_TX_Power: | Omit
readSFN_Indicator: | false
tx_DiversityIndicator: | false
| cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP) Omit
| NewIntraFreqCellSI_RSCP:
intraFreqCellID: | 1
| cellInfo: (CellInfoSI_RSCP)
cellIndividualOffset: | Omit
| referenceTimeDifferenceToCell: Omit
| modeSpecificInfo:
| fdd:
| primaryCPICH_Info:
primaryScramblingCode: | 150
primaryCPICH_TX_Power: | Omit
readSFN_Indicator: | true
tx_DiversityIndicator: | false
| cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP)
q_OffsetS_N: | 0
maxAllowedUL_TX_Power: | 21
| modeSpecificInfo:
| fdd:
q_QualMin: | -16
q_RxlevMin: | -58
| NewIntraFreqCellSI_RSCP:
intraFreqCellID: | 2
| cellInfo: (CellInfoSI_RSCP)
cellIndividualOffset: | Omit
| referenceTimeDifferenceToCell: Omit
| modeSpecificInfo:
| fdd:
| primaryCPICH_Info:
primaryScramblingCode: | 200
primaryCPICH_TX_Power: | Omit
readSFN_Indicator: | true
tx_DiversityIndicator: | false
| cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP)
q_OffsetS_N: | 0
maxAllowedUL_TX_Power: | 21
| modeSpecificInfo:
| fdd:
q_QualMin: | -16
q_RxlevMin: | -58
| intraFreqMeasQuantity:
filterCoefficient: | Omit
| modeSpecificInfo:
| fdd:
intraFreqMeasQuantity_FDD: | cpich_RSCP
| intraFreqReportingQuantityForRACH: Omit
maxReportedCellsOnRACH: | Omit
| reportingInfoForCellDCH:
| intraFreqReportingQuantity:
| activeSetReportingQuantities: (CellReportingQuantities)
dummy (SFN_SFN_OTD_Type): | noReport
cellIdentity_reportingIndicator: | true
cellSynchronisationInfoReportingIndicator: | false
| modeSpecificInfo:
| fdd:
cpich_Ec_N0_reportingIndicator: | false
cpich_RSCP_reportingIndicator: | true
pathloss_reportingIndicator: | false
| monitoredSetReportingQuantities: (CellReportingQuantities)
dummy (SFN_SFN_OTD_Type): | noReport
cellIdentity_reportingIndicator: | true
cellSynchronisationInfoReportingIndicator: | true
| modeSpecificInfo:
| fdd:
cpich_Ec_N0_reportingIndicator: | false
cpich_RSCP_reportingIndicator: | true
pathloss_reportingIndicator: | false
| detectedSetReportingQuantities: (CellReportingQuantities) Omit
| measurementReportingMode:
measurementReportTransferMode (TransferMode): | acknowledgedModeRLC
periodicalOrEventTrigger: | eventTrigger
| reportCriteria: (CellDCH_ReportCriteria)
| intraFreqReportingCriteria:
| eventCriteriaList: (IntraFreqEventCriteriaList)
| IntraFreqEventCriteria:
| event: (IntraFreqEvent)
| e1a: (Event1a)
triggeringCondition (TriggeringCondition2): | monitoredSetCellsOnly
reportingRange: | 5
| forbiddenAffectCellList: Omit
w: | 1
reportDeactivationThreshold: | t2
reportingAmount: | ra4
reportingInterval: | ri4
hysteresis: | 0
timeToTrigger: | ttt640
| reportingCellStatus:
withinActiveAndOrMonitoredUsedFreq (MaxNumberOfReportingCellsType1): | e3
| IntraFreqEventCriteria:
| event: (IntraFreqEvent)
| e1b: (Event1b)
triggeringCondition (TriggeringCondition1): | activeSetCellsOnly
reportingRange: | 5
| forbiddenAffectCellList: Omit
w: | 1
hysteresis: | 0
timeToTrigger: | ttt640
| reportingCellStatus:
withinActiveAndOrMonitoredUsedFreq (MaxNumberOfReportingCellsType1): | e3
| IntraFreqEventCriteria:
| event: (IntraFreqEvent)
| e1c: (Event1c)
replacementActivationThreshold: | t3
reportingAmount: | ra4
reportingInterval: | ri4
hysteresis: | 0
timeToTrigger: | ttt640
| reportingCellStatus:
withinActiveAndOrMonitoredUsedFreq (MaxNumberOfReportingCellsType1): | e3
| interFreqMeasurementSysInfo: (InterFreqMeasurementSysInfo_RSCP)
| interFreqCellInfoSI_List: (InterFreqCellInfoSI_List_RSCP)
| removedInterFreqCellList: Omit
| newInterFreqCellList: (NewInterFreqCellSI_List_RSCP)
| NewInterFreqCellSI_RSCP:
interFreqCellID: | 3
| frequencyInfo:
| modeSpecificInfo:
| fdd: (FrequencyInfoFDD)
uarfcn_UL (UARFCN): | 9663
uarfcn_DL (UARFCN): | 10613
| cellInfo: (CellInfoSI_RSCP)
cellIndividualOffset: | Omit
| referenceTimeDifferenceToCell: Omit
| modeSpecificInfo:
| fdd:
| primaryCPICH_Info:
primaryScramblingCode: | 200
primaryCPICH_TX_Power: | Omit
readSFN_Indicator: | false
tx_DiversityIndicator: | false
| cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP)
q_OffsetS_N: | 0
maxAllowedUL_TX_Power: | 21
| modeSpecificInfo:
| fdd:
q_QualMin: | -16
q_RxlevMin: | -58
| NewInterFreqCellSI_RSCP:
interFreqCellID: | 4
| frequencyInfo: Omit
| cellInfo: (CellInfoSI_RSCP)
cellIndividualOffset: | Omit
| referenceTimeDifferenceToCell: Omit
| modeSpecificInfo:
| fdd:
| primaryCPICH_Info:
primaryScramblingCode: | 300
primaryCPICH_TX_Power: | Omit
readSFN_Indicator: | false
tx_DiversityIndicator: | false
| cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP)
q_OffsetS_N: | 0
maxAllowedUL_TX_Power: | 21
| modeSpecificInfo:
| fdd:
q_QualMin: | -16
q_RxlevMin: | -58
| NewInterFreqCellSI_RSCP:
interFreqCellID: | 5
| frequencyInfo: Omit
| cellInfo: (CellInfoSI_RSCP)
cellIndividualOffset: | Omit
| referenceTimeDifferenceToCell: Omit
| modeSpecificInfo:
| fdd:
| primaryCPICH_Info:
primaryScramblingCode: | 350
primaryCPICH_TX_Power: | Omit
readSFN_Indicator: | false
tx_DiversityIndicator: | false
| cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP)
q_OffsetS_N: | 0
maxAllowedUL_TX_Power: | 21
| modeSpecificInfo:
| fdd:
q_QualMin: | -16
q_RxlevMin: | -58
| NewInterFreqCellSI_RSCP:
interFreqCellID: | 4
| frequencyInfo:
| modeSpecificInfo:
| fdd: (FrequencyInfoFDD)
uarfcn_UL (UARFCN): | 9713
uarfcn_DL (UARFCN): | 10663
| cellInfo: (CellInfoSI_RSCP)
cellIndividualOffset: | Omit
| referenceTimeDifferenceToCell: Omit
| modeSpecificInfo:
| fdd:
| primaryCPICH_Info:
primaryScramblingCode: | 150
primaryCPICH_TX_Power: | Omit
readSFN_Indicator: | false
tx_DiversityIndicator: | false
| cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP)
q_OffsetS_N: | 0
maxAllowedUL_TX_Power: | 21
| modeSpecificInfo:
| fdd:
q_QualMin: | -16
q_RxlevMin: | -58
| NewInterFreqCellSI_RSCP:
interFreqCellID: | 7
| frequencyInfo: Omit
| cellInfo: (CellInfoSI_RSCP)
cellIndividualOffset: | Omit
| referenceTimeDifferenceToCell: Omit
| modeSpecificInfo:
| fdd:
| primaryCPICH_Info:
primaryScramblingCode: | 450
primaryCPICH_TX_Power: | Omit
readSFN_Indicator: | false
tx_DiversityIndicator: | false
| cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP)
q_OffsetS_N: | 0
maxAllowedUL_TX_Power: | 21
| modeSpecificInfo:
| fdd:
q_QualMin: | -16
q_RxlevMin: | -58
| interRATMeasurementSysInfo: (InterRATMeasurementSysInfo_B) Omit

| trafficVolumeMeasSysInfo: Omit

| dummy: (UE_InternalMeasurementSysInfo) Omit

| nonCriticalExtensions: Omit

| Outputs:
BITSTRING: |
[0] | 00 | 10 | 00 | 00 | 11 | 01 | 10 | 01
[8] | 00 | 00 | 10 | 10 | 00 | 00 | 00 | 00
[16] | 10 | 00 | 11 | 00 | 10 | 00 | 01 | 00
[24] | 00 | 10 | 01 | 01 | 00 | 10 | 01 | 01
[32] | 10 | 10 | 01 | 10 | 00 | 11 | 10 | 01
[40] | 10 | 10 | 00 | 00 | 00 | 00 | 10 | 00
[48] | 10 | 00 | 10 | 10 | 01 | 10 | 01 | 00
[56] | 01 | 00 | 11 | 00 | 01 | 11 | 00 | 11
[64] | 01 | 00 | 00 | 00 | 00 | 00 | 00 | 10
[72] | 00 | 10 | 00 | 10 | 00 | 11 | 00 | 10
[80] | 01 | 01 | 01 | 01 | 00 | 00 | 00 | 01
[88] | 00 | 10 | 10 | 00 | 01 | 01 | 00 | 10
[96] | 10 | 10 | 00 | 01 | 10 | 00 | 01 | 00
[104] | 10 | 10 | 00 | 10 | 00 | 00 | 10 | 10
[112] | 00 | 01 | 00 | 00 | 11 | 00 | 00 | 10
[120] | 01 | 01 | 00 | 10 | 01 | 10 | 10 | 10
[128] | 10 | 00 | 01 | 10 | 00 | 01 | 00 | 10
[136] | 10 | 10 | 01 | 00 | 11 | 00 | 01 | 10
[144] | 11 | 00 | 10 | 11 | 01 | 11 | 11 | 11
[152] | 01 | 00 | 10 | 11 | 10 | 10 | 10 | 01
[160] | 01 | 00 | 11 | 00 | 10 | 00 | 00 | 01
[168] | 10 | 00 | 11 | 10 | 01 | 10 | 10 | 00
[176] | 00 | 00 | 00 | 10 | 00 | 10 | 00 | 01
[184] | 01 | 01 | 00 | 10 | 11 | 00 | 00 | 01
[192] | 10 | 00 | 11 | 10 | 01 | 10 | 10 | 00
[200] | 00 | 00 | 00 | 10 | 00 | 10 | 10 | 01
[208] | 01 | 01 | 01 | 01 | 11 | 10 | 00 | 01
[216] | 10 | 00 | 11 | 10 | 01 | 10 | 10 | 00
[224] | 00 | 00 | 00 | 11 | 00 | 10 | 00 | 11
[232] | 00 | 10 | 11 | 11 | 10 | 00 | 11 | 01
[240] | 00 | 11 | 01 | 00 | 11 | 10 | 01 | 01
[248] | 00 | 10 | 01 | 01 | 10 | 00 | 01 | 10
[256] | 00 | 11 | 10 | 01 | 10 | 10 | 00 | 00
[264] | 00 | 00 | 10 | 00 | 11 | 10 | 01 | 01
[272] | 01 | 11 | 00 | 00 | 10 | 00 | 01 | 10
[280] | 00 | 11 | 10 | 01 | 10 | 10 | 00 | 00
[288] | 00 | 00 |  |  |  |  |  |

#### MAC_DATA_REQ

RLC |  | MAC | @ 00:00:08.880

| Category: |  | Configuration
| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCCH
| CFN: |  | 129

| Message Details:
RLC PDU size (bits): | 48
RLC PDU (raw): |
[0] | 00 | 0E | 06 | 0F | 02 | 91 |  |

#### MAC_DATA_REQ

RLC |  | MAC | @ 00:00:08.880

| Category: |  | Configuration
| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCCH
| CFN: |  | 129

| Message Details:
RLC PDU size (bits): | 16
RLC PDU (raw): |
[0] | 00 | 00 |  |  |  |  |  |

#### MAC_DATA_REQ

RLC |  | MAC | @ 00:00:08.880

| Category: |  | Configuration
| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCCH
| CFN: |  | 129

| Message Details:
RLC PDU size (bits): | 16
RLC PDU (raw): |
[0] | 00 | 00 |  |  |  |  |  |

#### MAC_DATA_REQ

RLC |  | MAC | @ 00:00:08.880

| Category: |  | Configuration
| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCCH
| CFN: |  | 129

| Message Details:
RLC PDU size (bits): | 16
RLC PDU (raw): |
[0] | 00 | 00 |  |  |  |  |  |

#### MAC_DATA_REQ

RLC |  | MAC | @ 00:00:08.880

| Category: |  | Configuration
| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCCH
| CFN: |  | 129

| Message Details:
RLC PDU size (bits): | 56
RLC PDU (raw): |
[0] | 00 | 0E | 07 | 17 | 82 | 80 | 81 |

#### MAC_DATA_REQ

RLC |  | MAC | @ 00:00:08.880

| Category: |  | Configuration
| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCCH
| CFN: |  | 129

| Message Details:
RLC PDU size (bits): | 184
RLC PDU (raw): |
[0] | 00 | 0E | 27 | 17 | 82 | 80 | 81 | 1B
[8] | 7A | 00 | 00 | 00 | 05 | B8 | C0 | 00
[16] | 80 | 12 | 10 | 23 | FF | FF | F8 |

#### MAC_DATA_REQ

RLC |  | MAC | @ 00:00:08.880

| Category: |  | Configuration
| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCCH
| CFN: |  | 129

| Message Details:
RLC PDU size (bits): | 168
RLC PDU (raw): |
[0] | 00 | 0E | 27 | 17 | 82 | 80 | 81 | D3
[8] | 14 | 43 | 80 | 10 | 46 | 00 | 41 | 18
[16] | 01 | 04 | 60 | 08 | 21 |  |  |

#### MAC_DATA_REQ

RLC |  | MAC | @ 00:00:08.880

| Category: |  | Configuration
| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCCH
| CFN: |  | 129

| Message Details:
RLC PDU size (bits): | 168
RLC PDU (raw): |
[0] | 00 | 0E | 27 | 17 | 82 | 80 | 81 | 22
[8] | F0 | 00 | 00 | 00 | 0B | 71 | 80 | 01
[16] | 00 | 24 | 00 | 47 | 70 |  |  |

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:08.890

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 30
bcch_ModificationTime: | Omit

#### PHY_DATA_REQ

MAC |  | PHY | @ 00:00:08.890

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCH
| CFN: |  | 130

| Message Details:
SIB repetition period: | 64
SIB position: | 4
SIB size: | 246
SIB (raw): |
[0] | 00 | 0E | 06 | 0F | 02 | 91 | 80 | 07
[8] | 88 | 60 | 16 | DB | 62 | 00 | 43 | 08
[16] | 94 | 0B | 68 | 04 | 00 | E0 | 08 | 86
[24] | 42 | 99 | 0A | 00 | 30 | 11 | 14 | 00
| SIB (decoded):
| TB 0:
MAC SDU (246 bits): |
[0] | 00 | 0E | 06 | 0F | 02 | 91 | 80 | 07
[8] | 88 | 60 | 16 | DB | 62 | 00 | 43 | 08
[16] | 94 | 0B | 68 | 04 | 00 | E0 | 08 | 86
[24] | 42 | 99 | 0A | 00 | 30 | 11 | 14 |

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:08.900

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:08.900

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
noSegment: |

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA |  | RLC | @ 00:00:08.900

| Channel No: |  | 0 Name: BCCH

| Message Details:
| SIB repetition rate: 64
| SIB position: 60
| BCCH_BCH_Message:
| message:
| sfn_Prime: 0
| payload:
| noSegment: NULL
Layer 3 SDU: |
[0] | 00 | 00 |  |  |  |  |  |

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:08.900

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 27
bcch_ModificationTime: | Omit

#### MAC_DATA_REQ

RLC |  | MAC | @ 00:00:08.910

| Category: |  | Configuration
| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCCH
| CFN: |  | 132

| Message Details:
RLC PDU size (bits): | 16
RLC PDU (raw): |
[0] | 00 | 00 |  |  |  |  |  |

#### PHY_DATA_REQ

MAC |  | PHY | @ 00:00:08.910

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCH
| CFN: |  | 132

| Message Details:
SIB repetition period: | 64
SIB position: | 6
SIB size: | 246
SIB (raw): |
[0] | 00 | 00 | 06 | 0F | 02 | 91 | 80 | 07
[8] | 88 | 60 | 16 | DB | 62 | 00 | 43 | 08
[16] | 94 | 0B | 68 | 04 | 00 | E0 | 08 | 86
[24] | 42 | 99 | 0A | 00 | 30 | 11 | 14 | 00
| SIB (decoded):
| TB 0:
MAC SDU (246 bits): |
[0] | 00 | 00 | 06 | 0F | 02 | 91 | 80 | 07
[8] | 88 | 60 | 16 | DB | 62 | 00 | 43 | 08
[16] | 94 | 0B | 68 | 04 | 00 | E0 | 08 | 86
[24] | 42 | 99 | 0A | 00 | 30 | 11 | 14 |

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:08.920

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:08.920

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
| subsequentSegment:
sib_Type: | systemInformationBlockType11
segmentIndex: | 1
sib_Data_fixed: | 100001000011000010010100100110101010000110000100101010010011000110110010110111111101001011101010010100110010000001100011100110100000000010001000010101001011000001100011100110100000000010001010010101010111100001100011100110

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA |  | RLC | @ 00:00:08.920

| Channel No: |  | 0 Name: BCCH

| Message Details:
| SIB repetition rate: 64
| SIB position: 54
| BCCH_BCH_Message:
| message:
| sfn_Prime: 0
| payload:
| subsequentSegment:
| sib_Type: systemInformationBlockType11_SIB_Type [enum=11]
| segmentIndex: 1
| sib_Data_fixed: 100001000011000010010100100110101010000110000100101010010011000110110010110111111101001011101010010100110010000001100011100110100000000010001000010101001011000001100011100110100000000010001010010101010111100001100011100110

Layer 3 SDU: |
[0] | 00 | 04 | B0 | 84 | 30 | 94 | 9A | A1
[8] | 84 | A9 | 31 | B2 | DF | D2 | EA | 53
[16] | 20 | 63 | 9A | 00 | 88 | 54 | B0 | 63
[24] | 9A | 00 | 8A | 55 | 78 | 63 | 98 |

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:08.920

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 26
bcch_ModificationTime: | Omit

#### PHY_DATA_REQ

MAC |  | PHY | @ 00:00:08.930

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCH
| CFN: |  | 134

| Message Details:
SIB repetition period: | 64
SIB position: | 10
SIB size: | 246
SIB (raw): |
[0] | 00 | 00 | 06 | 0F | 02 | 91 | 80 | 07
[8] | 88 | 60 | 16 | DB | 62 | 00 | 43 | 08
[16] | 94 | 0B | 68 | 04 | 00 | E0 | 08 | 86
[24] | 42 | 99 | 0A | 00 | 30 | 11 | 14 | 00
| SIB (decoded):
| TB 0:
MAC SDU (246 bits): |
[0] | 00 | 00 | 06 | 0F | 02 | 91 | 80 | 07
[8] | 88 | 60 | 16 | DB | 62 | 00 | 43 | 08
[16] | 94 | 0B | 68 | 04 | 00 | E0 | 08 | 86
[24] | 42 | 99 | 0A | 00 | 30 | 11 | 14 |

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:08.940

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:08.940

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
| firstSegment:
sib_Type: | systemInformationBlockType11
seg_Count (SegCount): | 3
sib_Data_fixed: | 001000001101100100001010000000001000110010000100001001010010010110100110001110011010000000001000100010100110010001001100011100110100000000000010001000100011001001010101000000010010100001010010101000011000010010100010000010

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA |  | RLC | @ 00:00:08.940

| Channel No: |  | 0 Name: BCCH

| Message Details:
| SIB repetition rate: 64
| SIB position: 52
| BCCH_BCH_Message:
| message:
| sfn_Prime: 0
| payload:
| firstSegment:
| sib_Type: systemInformationBlockType11_SIB_Type [enum=11]
| seg_Count: 3
| sib_Data_fixed: 001000001101100100001010000000001000110010000100001001010010010110100110001110011010000000001000100010100110010001001100011100110100000000000010001000100011001001010101000000010010100001010010101000011000010010100010000010

Layer 3 SDU: |
[0] | 00 | 02 | B2 | 20 | D9 | 0A | 00 | 8C
[8] | 84 | 25 | 25 | A6 | 39 | A0 | 08 | 8A
[16] | 64 | 4C | 73 | 40 | 02 | 22 | 32 | 55
[24] | 01 | 28 | 52 | A1 | 84 | A2 | 08 |

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:08.940

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity:
| -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 29
bcch_ModificationTime: | Omit

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:08.950

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:08.950

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
| lastSegmentShort:
sib_Type: | systemInformationBlockType11
segmentIndex: | 2
sib_Data_variable: | 1000000000110010001100101111100011010011010011100101001001011000011000111001101000000000100011100101011100001000011000111001101000000000

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA |  | RLC | @ 00:00:08.950

| Channel No: |  | 0 Name: BCCH

| Message Details:
| SIB repetition rate: 64
| SIB position: 58
| BCCH_BCH_Message:
| message:
| sfn_Prime: 0
| payload:
| lastSegmentShort:
| sib_Type: systemInformationBlockType11_SIB_Type [enum=11]
| segmentIndex: 2
| sib_Data_variable: 1000000000110010001100101111100011010011010011100101001001011000011000111001101000000000100011100101011100001000011000111001101000000000

Layer 3 SDU: |
[0] | 00 | 06 | B1 | 87 | 80 | 32 | 32 | F8
[8] | D3 | 4E | 52 | 58 | 63 | 9A | 00 | 8E
[16] | 57 | 08 | 63 | 9A | 00 |  |  |

#### o_SIB_PER_Encoding

RRC |  | RRC | @ 00:00:08.950

| Category: |  | TSO

| Message Details:
| Inputs:
| SIB:
| sIB12: (SysInfoType12)
| fach_MeasurementOccasionInfo: Omit
| measurementControlSysInfo:
| use_of_HCS:
| hcs_not_used:
| cellSelectQualityMeasure:
| cpich_RSCP:
| intraFreqMeasurementSysInfo: (IntraFreqMeasurementSysInfo_RSCP)
intraFreqMeasurementID (MeasurementIdentity): | Omit
| intraFreqCellInfoSI_List: (IntraFreqCellInfoSI_List_RSCP)
| removedIntraFreqCellList: Omit
| newIntraFreqCellList: (NewIntraFreqCellSI_List_RSCP)
| NewIntraFreqCellSI_RSCP:
intraFreqCellID: | 1
| cellInfo: (CellInfoSI_RSCP)
cellIndividualOffset: | Omit
| referenceTimeDifferenceToCell: Omit
| modeSpecificInfo:
| fdd:
| primaryCPICH_Info:
primaryScramblingCode: | 150

primaryCPICH_TX_Power: | Omit
readSFN_Indicator: | true
tx_DiversityIndicator: | false

| cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP)
q_OffsetS_N: | 0
maxAllowedUL_TX_Power: | 21
| modeSpecificInfo:
| fdd:
q_QualMin: | -16
q_RxlevMin: | -58

| NewIntraFreqCellSI_RSCP:
intraFreqCellID: | 2
| cellInfo: (CellInfoSI_RSCP)
cellIndividualOffset: | Omit
| referenceTimeDifferenceToCell: Omit
| modeSpecificInfo:
| fdd:
| primaryCPICH_Info:
primaryScramblingCode: | 200

primaryCPICH_TX_Power: | Omit
readSFN_Indicator: | true
tx_DiversityIndicator: | false

| cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP)
q_OffsetS_N: | 0
maxAllowedUL_TX_Power: | 21
| modeSpecificInfo:
| fdd:
q_QualMin: | -16
q_RxlevMin: | -58

| intraFreqMeasQuantity:
filterCoefficient: | Omit
| modeSpecificInfo:
| fdd:
intraFreqMeasQuantity_FDD: | cpich_RSCP

| intraFreqReportingQuantityForRACH: Omit

maxReportedCellsOnRACH: | Omit

| reportingInfoForCellDCH:
| intraFreqReportingQuantity:
| activeSetReportingQuantities: (CellReportingQuantities)
dummy (SFN_SFN_OTD_Type): | noReport
cellIdentity_reportingIndicator: | true
cellSynchronisationInfoReportingIndicator: | false
| modeSpecificInfo:
| fdd:
cpich_Ec_N0_reportingIndicator: | false
cpich_RSCP_reportingIndicator: | true
pathloss_reportingIndicator: | false

| monitoredSetReportingQuantities: (CellReportingQuantities)
dummy (SFN_SFN_OTD_Type): | noReport
cellIdentity_reportingIndicator: | true
cellSynchronisationInfoReportingIndicator: | true
| modeSpecificInfo:
| fdd:
cpich_Ec_N0_reportingIndicator: | false
cpich_RSCP_reportingIndicator: | true
pathloss_reportingIndicator: | false

| detectedSetReportingQuantities: (CellReportingQuantities) Omit

| measurementReportingMode:
measurementReportTransferMode (TransferMode): | acknowledgedModeRLC
periodicalOrEventTrigger: | eventTrigger

| reportCriteria: (CellDCH_ReportCriteria)
| intraFreqReportingCriteria:
| eventCriteriaList: (IntraFreqEventCriteriaList)
| IntraFreqEventCriteria:
| event: (IntraFreqEvent)
| e1a: (Event1a)
triggeringCondition (TriggeringCondition2): | monitoredSetCellsOnly
reportingRange: | 5
| forbiddenAffectCellList: Omit
w: | 1
reportDeactivationThreshold: | t2
reportingAmount: | ra4
reportingInterval: | noPeriodicalreporting

hysteresis: | 0
timeToTrigger: | ttt640

| reportingCellStatus:
withinActiveAndOrMonitoredUsedFreq (MaxNumberOfReportingCellsType1): | e3

| IntraFreqEventCriteria:
| event: (IntraFreqEvent)
| e1b: (Event1b)
triggeringCondition (TriggeringCondition1): | activeSetCellsOnly
reportingRange: | 5
| forbiddenAffectCellList: Omit
w: | 1

hysteresis: | 0
timeToTrigger: | ttt640

| reportingCellStatus:
withinActiveAndOrMonitoredUsedFreq (MaxNumberOfReportingCellsType1): | e3

| IntraFreqEventCriteria:
| event: (IntraFreqEvent)
| e1c: (Event1c)
replacementActivationThreshold: | t3
reportingAmount: | ra4
reportingInterval: | ri4

hysteresis: | 0
timeToTrigger: | ttt640

| reportingCellStatus:
withinActiveAndOrMonitoredUsedFreq (MaxNumberOfReportingCellsType1): | e3

| interFreqMeasurementSysInfo: (InterFreqMeasurementSysInfo_RSCP)
| interFreqCellInfoSI_List: (InterFreqCellInfoSI_List_RSCP)
| removedInterFreqCellList: Omit
| newInterFreqCellList: (NewInterFreqCellSI_List_RSCP)
| NewInterFreqCellSI_RSCP:
interFreqCellID: | 3
| frequencyInfo:
| modeSpecificInfo:
| fdd: (FrequencyInfoFDD)
uarfcn_UL (UARFCN): | 9663
uarfcn_DL (UARFCN): | 10613

| cellInfo: (CellInfoSI_RSCP)
cellIndividualOffset: | Omit
| referenceTimeDifferenceToCell: Omit
| modeSpecificInfo:
| fdd:
| primaryCPICH_Info:
primaryScramblingCode: | 200

primaryCPICH_TX_Power: | Omit
readSFN_Indicator: | true
tx_DiversityIndicator: | false

| cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP)
q_OffsetS_N: | 0
maxAllowedUL_TX_Power: | 21
| modeSpecificInfo:
| fdd:
q_QualMin: | -16
q_RxlevMin: | -58

| NewInterFreqCellSI_RSCP:
interFreqCellID: | 4
| frequencyInfo: Omit
| cellInfo: (CellInfoSI_RSCP)
cellIndividualOffset: | Omit
| referenceTimeDifferenceToCell: Omit
| modeSpecificInfo:
| fdd:
| primaryCPICH_Info:
primaryScramblingCode: | 300

primaryCPICH_TX_Power: | Omit
readSFN_Indicator: | true
tx_DiversityIndicator: | false

| cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP)
q_OffsetS_N: | 0
maxAllowedUL_TX_Power: | 21
| modeSpecificInfo:
| fdd:
q_QualMin: | -16
q_RxlevMin: | -58

| NewInterFreqCellSI_RSCP:
interFreqCellID: | 5
| frequencyInfo: Omit
| cellInfo: (CellInfoSI_RSCP)
cellIndividualOffset: | Omit
| referenceTimeDifferenceToCell: Omit
| modeSpecificInfo:
| fdd:
| primaryCPICH_Info:
primaryScramblingCode: | 350

primaryCPICH_TX_Power: | Omit
readSFN_Indicator: | true
tx_DiversityIndicator: | false

| cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP)
q_OffsetS_N: | 0
maxAllowedUL_TX_Power: | 21
| modeSpecificInfo:
| fdd:
q_QualMin: | -16
q_RxlevMin: | -58

| NewInterFreqCellSI_RSCP:
interFreqCellID: | 4
| frequencyInfo:
| modeSpecificInfo:
| fdd: (FrequencyInfoFDD)
uarfcn_UL (UARFCN): | 9713
uarfcn_DL (UARFCN): | 10663

| cellInfo: (CellInfoSI_RSCP)
cellIndividualOffset: | Omit
| referenceTimeDifferenceToCell: Omit
| modeSpecificInfo:
| fdd:
| primaryCPICH_Info:
primaryScramblingCode: | 150

primaryCPICH_TX_Power: | Omit
readSFN_Indicator: | true
tx_DiversityIndicator: | false

| cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP)
q_OffsetS_N: | 0
maxAllowedUL_TX_Power: | 21
| modeSpecificInfo:
| fdd:
q_QualMin: | -16
q_RxlevMin: | -58

| NewInterFreqCellSI_RSCP:
interFreqCellID: | 7
| frequencyInfo: Omit
| cellInfo: (CellInfoSI_RSCP)
cellIndividualOffset: | Omit
| referenceTimeDifferenceToCell: Omit
| modeSpecificInfo:
| fdd:
| primaryCPICH_Info:
primaryScramblingCode: | 450

primaryCPICH_TX_Power: | Omit
readSFN_Indicator: | true
tx_DiversityIndicator: | false

| cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP)
q_OffsetS_N: | 0
maxAllowedUL_TX_Power: | 21
| modeSpecificInfo:
| fdd:
q_QualMin: | -16
q_RxlevMin: | -58

| interRATMeasurementSysInfo: (InterRATMeasurementSysInfo_B) Omit

| trafficVolumeMeasSysInfo: Omit

| dummy: (UE_InternalMeasurementSysInfo) Omit

| nonCriticalExtensions: Omit

| Outputs:
BITSTRING: |
[0] | 00 | 00 | 00 | 01 | 10 | 11 | 00 | 10
[8] | 00 | 00 | 11 | 00 | 00 | 10 | 01 | 01
[16] | 00 | 10 | 01 | 01 | 10 | 10 | 01 | 10
[24] | 00 | 11 | 10 | 01 | 10 | 10 | 00 | 00
[32] | 00 | 00 | 10 | 00 | 10 | 00 | 10 | 10
[40] | 01 | 10 | 01 | 00 | 01 | 00 | 11 | 00
[48] | 01 | 11 | 00 | 11 | 01 | 00 | 00 | 00
[56] | 00 | 00 | 00 | 10 | 00 | 10 | 00 | 10
[64] | 00 | 11 | 00 | 10 | 01 | 01 | 01 | 01
[72] | 00 | 00 | 00 | 01 | 00 | 10 | 10 | 00
[80] | 01 | 01 | 00 | 10 | 00 | 00 | 00 | 01
[88] | 10 | 00 | 01 | 00 | 10 | 10 | 00 | 10
[96] | 00 | 00 | 10 | 10 | 00 | 01 | 00 | 00
[104] | 11 | 00 | 00 | 10 | 01 | 01 | 00 | 10
[112] | 01 | 10 | 10 | 10 | 10 | 00 | 01 | 10
[120] | 00 | 01 | 00 | 10 | 10 | 10 | 01 | 00
[128] | 11 | 00 | 01 | 10 | 11 | 00 | 10 | 11
[136] | 01 | 11 | 11 | 11 | 01 | 00 | 10 | 11
[144] | 10 | 10 | 10 | 01 | 01 | 00 | 11 | 00
[152] | 10 | 00 | 10 | 01 | 10 | 00 | 11 | 10
[160] | 01 | 10 | 10 | 00 | 00 | 00 | 00 | 10
[168] | 00 | 10 | 00 | 01 | 01 | 01 | 00 | 10
[176] | 11 | 00 | 10 | 01 | 10 | 00 | 11 | 10
[184] | 01 | 10 | 10 | 00 | 00 | 00 | 00 | 10
[192] | 00 | 10 | 10 | 01 | 01 | 01 | 01 | 01
[200] | 11 | 10 | 10 | 01 | 10 | 00 | 11 | 10
[208] | 01 | 10 | 10 | 00 | 00 | 00 | 00 | 11
[216] | 00 | 10 | 00 | 11 | 00 | 10 | 11 | 11
[224] | 10 | 00 | 11 | 01 | 00 | 11 | 01 | 00
[232] | 11 | 10 | 01 | 01 | 00 | 10 | 01 | 01
[240] | 10 | 10 | 01 | 10 | 00 | 11 | 10 | 01
[248] | 10 | 10 | 00 | 00 | 00 | 00 | 10 | 00
[256] | 11 | 10 | 01 | 01 | 01 | 11 | 00 | 00
[264] | 10 | 10 | 01 | 10 | 00 | 11 | 10 | 01
[272] | 10 | 10 | 00 | 00 | 00 | 00 |  |

#### PHY_DATA_REQ

MAC |  | PHY | @ 00:00:08.950

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCH
| CFN: |  | 136

| Message Details:
SIB repetition period: | 64
SIB position: | 12
SIB size: | 246
SIB (raw): |
[0] | 00 | 00 | 06 | 0F | 02 | 91 | 80 | 07
[8] | 88 | 60 | 16 | DB | 62 | 00 | 43 | 08
[16] | 94 | 0B | 68 | 04 | 00 | E0 | 08 | 86
[24] | 42 | 99 | 0A | 00 | 30 | 11 | 14 | 00

| SIB (decoded):
| TB 0:
MAC SDU (246 bits): |
[0] | 00 | 00 | 06 | 0F | 02 | 91 | 80 | 07
[8] | 88 | 60 | 16 | DB | 62 | 00 | 43 | 08
[16] | 94 | 0B | 68 | 04 | 00 | E0 | 08 | 86
[24] | 42 | 99 | 0A | 00 | 30 | 11 | 14 |

#### PHY_DATA_REQ

MAC |  | PHY | @ 00:00:08.970

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCH
| CFN: |  | 138

| Message Details:
SIB repetition period:
| 64
SIB position: | 30
SIB size: | 246
SIB (raw): |
[0]
| 00 | 0E | 07 | 17 | 82 | 80 | 81 | 07
[8] | 88 | 60 | 16 | DB | 62 | 00 | 43 | 08
[16] | 94 | 0B | 68 | 04 | 00 | E0 | 08 | 86
[24] | 42 | 99 | 0A | 00 | 30 | 11 | 14 | 00

| SIB (decoded):
| TB 0:
MAC SDU (246 bits): |
[0] | 00 | 0E | 07 | 17 | 82 | 80 | 81 | 07
[8] | 88 | 60 | 16 | DB | 62 | 00 | 43 | 08
[16] | 94 | 0B | 68 | 04 | 00 | E0 | 08 | 86
[24] | 42 | 99 | 0A | 00 | 30 | 11 | 14 |

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:08.980

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0

| routingInfo:
rB_Identity: | -1

ratType: | fdd

| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 13
bcch_ModificationTime: | Omit

#### PHY_DATA_REQ

MAC |  | PHY | @ 00:00:08.990

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCH
| CFN: |  | 140

| Message Details:
SIB repetition period: | 64
SIB position: | 14
SIB size: | 246
SIB (raw): |
[0] | 00 | 0E | 27 | 17 | 82 | 80 | 81 | 1B
[8] | 7A | 00 | 00 | 00 | 05 | B8 | C0 | 00
[16] | 80 | 12 | 10 | 23 | FF | FF | F8 | 86
[24] | 42 | 99 | 0A | 00 | 30 | 11 | 14 | 00

| SIB (decoded):
| TB 0:
MAC SDU (246 bits): |
[0] | 00 | 0E | 27 | 17 | 82 | 80 | 81 | 1B
[8] | 7A | 00 | 00 | 00 | 05 | B8 | C0 | 00
[16] | 80 | 12 | 10 | 23 | FF | FF | F8 | 86
[24] | 42 | 99 | 0A | 00 | 30 | 11 | 14 |

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:09.000

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0

| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:09.000

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details: |  | RLC_TR_DATA_REQ: | cellId: | 0

| routingInfo: | rB_Identity: | -1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

| payload:
| subsequentSegment:
sib_Type: | systemInformationBlockType12
segmentIndex: | 1
sib_Data_fixed: | 100110101010000110000100101010010011000110110010110111111101001011101010010100110010001001100011100110100000000010001000010101001011001001100011100110100000000010001010010101010111101001100011100110100000000011001000110010

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA |  | RLC | @ 00:00:09.000

| Channel No: |  | 0 Name: BCCH

| Message Details: |  | SIB repetition rate: 64

SIB position: 26

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

subsequentSegment:

sib_Type: systemInformationBlockType12_SIB_Type [enum=12]

segmentIndex: 1

sib_Data_fixed: 100110101010000110000100101010010011000110110010110111111101001011101010010100110010001001100011100110100000000010001000010101001011001001100011100110100000000010001010010101010111101001100011100110100000000011001000110010

Layer 3 SDU:

[0]00 04 C0 9A A1 84 A9 31
[8]B2 DF D2 EA 53 22 63 9A
[16]00 88 54 B2 63 9A 00 8A
[24]55 7A 63 9A 00 C8 C8

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:00:09.000

Channel ID: RbBcch
Cell ID: 0

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:0

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:11
bcch_ModificationTime: Omit

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:00:09.010

Channel ID: RbBcch
Cell ID: 0

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:0

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:00:09.010

Channel ID: RbBcch
Cell ID: 0

Message Details:

RLC_TR_DATA_REQ:

cellId:0

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

firstSegment:

sib_Type:systemInformationBlockType12
seg_Count (SegCount):3
sib_Data_fixed:000000011011001000001100001001010010010110100110001110011010000000001000100010100110010001001100011100110100000000000010001000100011001001010101000000010010100001010010000000011000010010100010000010100001000011000010010100

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:00:09.010

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 22

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

firstSegment:

sib_Type: systemInformationBlockType12_SIB_Type [enum=12]

seg_Count: 3

sib_Data_fixed: 000000011011001000001100001001010010010110100110001110011010000000001000100010100110010001001100011100110100000000000010001000100011001001010101000000010010100001010010000000011000010010100010000010100001000011000010010100

Layer 3 SDU:

[0]00 02 C2 01 B2 0C 25 25
[8]A6 39 A0 08 8A 64 4C 73
[16]40 02 22 32 55 01 28 52
[24]01 84 A2 0A 10 C2 50

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:00:09.010

Channel ID: RbBcch
Cell ID: 0

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:0

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:15
bcch_ModificationTime: Omit

#### PHY_DATA_REQ

MAC PHY @ 00:00:09.010

BTS unit: 1:1
Channel No: 0 Name: BCH
CFN: 142

Message Details:

SIB repetition period:64
SIB position:46
SIB size:246
SIB (raw):

[0]00 0E 27 17 82 80 81 D3
[8]14 43 80 10 46 00 41 18
[16]01 04 60 08 21 FF F8 86
[24]42 99 0A 00 30 11 14 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 0E 27 17 82 80 81 D3
[8]14 43 80 10 46 00 41 18
[16]01 04 60 08 21 FF F8 86
[24]42 99 0A 00 30 11 14

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:00:09.030

Channel ID: RbBcch
Cell ID: 0

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:0

routingInfo:

rB_Identity:-1

#### o_SIB_PER_Encoding

RRC RRC @ 00:00:09.030

Category: TSO

Message Details:

Inputs:

SIB:

sIB7: (SysInfoType7)

modeSpecificInfo:

fdd:

ul_Interference:-100

prach_Information_SIB5_List: (DynamicPersistenceLevelList)

DynamicPersistenceLevel:2

prach_Information_SIB6_List: (DynamicPersistenceLevelList)

DynamicPersistenceLevel:2

expirationTimeFactor: Omit

nonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]10 00 00 10 10 00 00 00
[8]10 00 00 01

#### RLC_TR_DATA_REQ

RRC LLA @ 00:00:09.030

Channel ID: RbBcch
Cell ID: 0

Message Details:

RLC_TR_DATA_REQ:

cellId:0

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

completeSIB_List:

CompleteSIBshort:

sib_Type:systemInformationBlockType7
sib_Data_variable:100000101000000010000001

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:00:09.030

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 30

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

completeSIB_List:

CompleteSIB_List.element:

sib_Type: systemInformationBlockType7_SIB_Type [enum=7]

sib_Data_variable: 100000101000000010000001

Layer 3 SDU:

[0]00 0E 07 17 82 80 81

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:00:09.030

Channel ID: RbBcch
Cell ID: 0

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:0

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:14
bcch_ModificationTime: Omit

#### MAC_DATA_REQ

RLC MAC @ 00:00:09.030

Category: Configuration
BTS unit: 1:1
Channel No: 0 Name: BCCH
CFN: 144

Message Details:

RLC PDU size (bits):248
RLC PDU (raw):

[0]00 04 B0 84 30 94 9A A1
[8]84 A9 31 B2 DF D2 EA 53
[16]20 63 9A 00 88 54 B0 63
[24]9A 00 8A 55 78 63 98

#### MAC_DATA_REQ

RLC MAC @ 00:00:09.030

Category: Configuration
BTS unit: 1:1
Channel No: 0 Name: BCCH
CFN: 144

Message Details:

RLC PDU size (bits):248
RLC PDU (raw):

[0]00 02 B2 20 D9 0A 00 8C
[8]84 25 25 A6 39 A0 08 8A
[16]64 4C 73 40 02 22 32 55
[24]01 28 52 A1 84 A2 08

#### MAC_DATA_REQ

RLC MAC @ 00:00:09.030

Category: Configuration
BTS unit: 1:1
Channel No: 0 Name: BCCH
CFN: 144

Message Details:

RLC PDU size (bits):168
RLC PDU (raw):

[0]00 06 B1 87 80 32 32 F8
[8]D3 4E 52 58 63 9A 00 8E
[16]57 08 63 9A 00

#### MAC_DATA_REQ

RLC MAC @ 00:00:09.030

Category: Configuration
BTS unit: 1:1
Channel No: 0 Name: BCCH
CFN: 144

Message Details:

RLC PDU size (bits):248
RLC PDU (raw):

[0]00 04 C0 9A A1 84 A9 31
[8]B2 DF D2 EA 53 22 63 9A
[16]00 88 54 B2 63 9A 00 8A
[24]55 7A 63 9A 00 C8 C8

#### MAC_DATA_REQ

RLC MAC @ 00:00:09.030

Category: Configuration
BTS unit: 1:1
Channel No: 0 Name: BCCH
CFN: 144

Message Details:

RLC PDU size (bits):248
RLC PDU (raw):

[0]00 02 C2 01 B2 0C 25 25
[8]A6 39 A0 08 8A 64 4C 73
[16]40 02 22 32 55 01 28 52
[24]01 84 A2 0A 10 C2 50

#### PHY_DATA_REQ

MAC PHY @ 00:00:09.030

BTS unit: 1:1
Channel No: 0 Name: BCH
CFN: 144

Message Details:

SIB repetition period:64
SIB position:62
SIB size:246
SIB (raw):

[0]00 0E 27 17 82 80 81 22
[8]F0 00 00 00 0B 71 80 01
[16]00 24 00 47 70 FF F8 86
[24]42 99 0A 00 30 11 14 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 0E 27 17 82 80 81 22
[8]F0 00 00 00 0B 71 80 01
[16]00 24 00 47 70 FF F8 86
[24]42 99 0A 00 30 11 14

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:00:09.040

Channel ID: RbBcch
Cell ID: 0

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:0

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:00:09.040

Channel ID: RbBcch
Cell ID: 0

Message Details:

RLC_TR_DATA_REQ:

cellId:0

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

lastSegmentShort:

sib_Type:systemInformationBlockType12
segmentIndex:2
sib_Data_variable:1111100011010011010011100101001001011010011000111001101000000000100011100101011100001010011000111001101000000000

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:00:09.040

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 28

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

lastSegmentShort:

sib_Type: systemInformationBlockType12_SIB_Type [enum=12]

segmentIndex: 2

sib_Data_variable: 1111100011010011010011100101001001011010011000111001101000000000100011100101011100001010011000111001101000000000

Layer 3 SDU:

[0]00 06 C1 6F F8 D3 4E 52
[8]5A 63 9A 00 8E 57 0A 63
[16]9A 00

#### o_SIB_PER_Encoding

RRC RRC @ 00:00:09.040

Category: TSO

Message Details:

Inputs:

SIB:

sIB18: (SysInfoType18)

idleModePLMNIdentities: (PLMNIdentitiesOfNeighbourCells)

plmnsOfIntraFreqCellsList: Omit

plmnsOfInterFreqCellsList:

:

plmn_Identity:

mcc:

Digit:0
Digit:0
Digit:2

mnc:

Digit:1
Digit:1

:

plmn_Identity:

mcc:

Digit:0
Digit:0
Digit:2

mnc:

Digit:1
Digit:1

:

plmn_Identity:

mcc:

Digit:0
Digit:0
Digit:2

mnc:

Digit:1
Digit:1

:

plmn_Identity:

mcc:

Digit:0
Digit:0
Digit:4

mnc:

Digit:2
Digit:1

plmnsOfInterRATCellsList: Omit

connectedModePLMNIdentities: (PLMNIdentitiesOfNeighbourCells) Omit

nonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]10 00 10 00 01 11 00 00
[8]00 00 00 10 00 00 10 00
[16]11 00 00 00 00 00 10 00
[24]00 10 00 11 00 00 00 00
[32]00 10 00 00 10 00 11 00
[40]00 00 00 01 00 00 01 00
[48]00 1

#### o_SIB_PER_Encoding

RRC RRC @ 00:00:09.040

Category: TSO

Message Details:

Inputs:

SIB:

sIB7: (SysInfoType7)

modeSpecificInfo:

fdd:

ul_Interference:-100

prach_Information_SIB5_List: (DynamicPersistenceLevelList)

DynamicPersistenceLevel:2

prach_Information_SIB6_List: (DynamicPersistenceLevelList)

DynamicPersistenceLevel:2

expirationTimeFactor: Omit

nonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]10 00 00 10 10 00 00 00
[8]10 00 00 01

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:00:09.040

Channel ID: RbBcch
Cell ID: 0

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:0

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:23
bcch_ModificationTime: Omit

#### PHY_DATA_REQ

MAC PHY @ 00:00:09.050

BTS unit: 1:1
Channel No: 0 Name: BCH
CFN: 146

Message Details:

SIB repetition period:64
SIB position:60
SIB size:246
SIB (raw):

[0]00 00 27 17 82 80 81 22
[8]F0 00 00 00 0B 71 80 01
[16]00 24 00 47 70 FF F8 86
[24]42 99 0A 00 30 11 14 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 00 27 17 82 80 81 22
[8]F0 00 00 00 0B 71 80 01
[16]00 24 00 47 70 FF F8 86
[24]42 99 0A 00 30 11 14

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:00:09.060

Channel ID: RbBcch
Cell ID: 0

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:0

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:00:09.060

Channel ID: RbBcch
Cell ID: 0

Message Details:

RLC_TR_DATA_REQ:

cellId:0

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

completeSIB_List:

CompleteSIBshort:

sib_Type:systemInformationBlockType7
sib_Data_variable:100000101000000010000001

CompleteSIBshort:

sib_Type:systemInformationBlockType18
sib_Data_variable:100010000111000000000010000010001100000000001000001000110000000000100000100011000000000100000100001

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:00:09.060

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 46

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

completeSIB_List:

CompleteSIB_List.element:

sib_Type: systemInformationBlockType7_SIB_Type [enum=7]

sib_Data_variable: 100000101000000010000001

CompleteSIB_List.element:

sib_Type: systemInformationBlockType18_SIB_Type [enum=26]

sib_Data_variable: 100010000111000000000010000010001100000000001000001000110000000000100000100011000000000100000100001

Layer 3 SDU:

[0]00 0E 27 17 82 80 81 D3
[8]14 43 80 10 46 00 41 18
[16]01 04 60 08 21

#### o_SIB_PER_Encoding

RRC RRC @ 00:00:09.060

Category: TSO

Message Details:

Inputs:

SIB:

sB1: (SysInfoTypeSB1)

sib_ReferenceList:

SchedulingInformationSIB:

sib_Type: (SIB_TypeAndTag)

sysInfoType6 (CellValueTag):2

scheduling: (SchedulingInformation)

scheduling:

segCount: Omit

sib_Pos:

rep64:2

sib_PosOffsetInfo: (SibOFF_List) Omit

SchedulingInformationSIB:

sib_Type: (SIB_TypeAndTag)

sysInfoType7:

scheduling: (SchedulingInformation)

scheduling:

segCount: Omit

sib_Pos:

rep16:7

sib_PosOffsetInfo: (SibOFF_List) Omit

SchedulingInformationSIB:

sib_Type: (SIB_TypeAndTag)

sysInfoType11 (CellValueTag):2

scheduling: (SchedulingInformation)

scheduling:

segCount:3

sib_Pos:

rep64:26

sib_PosOffsetInfo: (SibOFF_List)

SibOFF:so2
SibOFF:so4

SchedulingInformationSIB:

sib_Type: (SIB_TypeAndTag)

sysInfoType12 (CellValueTag):2

scheduling: (SchedulingInformation)

scheduling:

segCount:3

sib_Pos:

rep64:11

sib_PosOffsetInfo: (SibOFF_List)

SibOFF:so4
SibOFF:so2

SchedulingInformationSIB:

sib_Type: (SIB_TypeAndTag)

sysInfoType18 (CellValueTag):2

scheduling: (SchedulingInformation)

scheduling:

segCount: Omit

sib_Pos:

rep64:23

sib_PosOffsetInfo: (SibOFF_List) Omit

nonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]00 01 00 00 10 10 10 00
[8]10 00 00 10 00 11 00 00
[16]01 01 11 01 01 00 11 10
[24]01 00 10 01 10 10 00 01
[32]00 00 00 01 01 01 10 11
[40]10 01 00 10 00 10 11 00
[48]01 00 01 00 00 11 00 10
[56]10 00 10 01 01 11

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:00:09.060

Channel ID: RbBcch
Cell ID: 0

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:0

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:4
sg_POS:1
bcch_ModificationTime: Omit

#### PHY_DATA_REQ

MAC PHY @ 00:00:09.070

BTS unit: 1:1
Channel No: 0 Name: BCH
CFN: 148

Message Details:

SIB repetition period:64
SIB position:54
SIB size:246
SIB (raw):

[0]00 04 B0 84 30 94 9A A1
[8]84 A9 31 B2 DF D2 EA 53
[16]20 63 9A 00 88 54 B0 63
[24]9A 00 8A 55 78 63 98 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 04 B0 84 30 94 9A A1
[8]84 A9 31 B2 DF D2 EA 53
[16]20 63 9A 00 88 54 B0 63
[24]9A 00 8A 55 78 63 98

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:00:09.080

Channel ID: RbBcch
Cell ID: 0

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:0

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:00:09.080

Channel ID: RbBcch
Cell ID: 0

Message Details:

RLC_TR_DATA_REQ:

cellId:0

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

completeSIB_List:

CompleteSIBshort:

sib_Type:schedulingBlock1
sib_Data_variable:0001000010101000100000100011000001011101010011100100100110100001000000010101101110010010001011000100010000110010100010010111

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:00:09.080

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 16

SIB position: 2

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

completeSIB_List:

CompleteSIB_List.element:

sib_Type: schedulingBlock1_SIB_Type [enum=27]

sib_Data_variable: 0001000010101000100000100011000001011101010011100100100110100001000000010101101110010010001011000100010000110010100010010111

Layer 3 SDU:

[0]00 0E 1B 7B 10 A8 82 30
[8]5D 4E 49 A1 01 5B 92 2C
[16]44 32 89 70

#### o_SIB_PER_Encoding

RRC RRC @ 00:00:09.090

Category: TSO

Message Details:

Inputs:

SIB:

mIB: (MasterInformationBlock)

mib_ValueTag:1

plmn_Type:

gsm_MAP:

plmn_Identity:

mcc:

Digit:0
Digit:0
Digit:1

mnc:

Digit:0
Digit:1

sibSb_ReferenceList:

SchedulingInformationSIBSb:

sibSb_Type: (SIBSb_TypeAndTag)

sysInfoTypeSB1 (CellValueTag):2

scheduling: (SchedulingInformation)

scheduling:

segCount: Omit

sib_Pos:

rep16:1

sib_PosOffsetInfo: (SibOFF_List) Omit

SchedulingInformationSIBSb:

sibSb_Type: (SIBSb_TypeAndTag)

sysInfoType1 (PLMN_ValueTag):2

scheduling: (SchedulingInformation)

scheduling:

segCount: Omit

sib_Pos:

rep64:10

sib_PosOffsetInfo: (SibOFF_List) Omit

SchedulingInformationSIBSb:

sibSb_Type: (SIBSb_TypeAndTag)

sysInfoType2 (CellValueTag):2

scheduling: (SchedulingInformation)

scheduling:

segCount: Omit

sib_Pos:

rep64:10

sib_PosOffsetInfo: (SibOFF_List) Omit

SchedulingInformationSIBSb:

sibSb_Type: (SIBSb_TypeAndTag)

sysInfoType3 (CellValueTag):2

scheduling: (SchedulingInformation)

scheduling:

segCount: Omit

sib_Pos:

rep64:7

sib_PosOffsetInfo: (SibOFF_List) Omit

SchedulingInformationSIBSb:

sibSb_Type: (SIBSb_TypeAndTag)

sysInfoType4 (CellValueTag):2

scheduling: (SchedulingInformation)

scheduling:

segCount: Omit

sib_Pos:

rep64:31

sib_PosOffsetInfo: (SibOFF_List) Omit

SchedulingInformationSIBSb:

sibSb_Type: (SIBSb_TypeAndTag)

sysInfoType5 (CellValueTag):2

scheduling: (SchedulingInformation)

scheduling:

segCount:3

sib_Pos:

rep64:18

sib_PosOffsetInfo: (SibOFF_List)

SibOFF:so2
SibOFF:so4

nonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]00 00 00 00 00 00 00 00
[8]01 00 00 00 00 10 01 01
[16]10 10 10 10 00 01 00 01
[24]00 00 00 00 00 00 10 00
[32]10 00 10 10 00 00 10 10
[40]00 10 00 10 10 00 01 00
[48]10 00 10 00 01 11 00 01
[56]10 10 00 10 01 11 11 00
[64]10 00 11 10 01 00 10 01
[72]00 10 00 01 00 00 00 01

#### PHY_DATA_REQ

MAC PHY @ 00:00:09.090

BTS unit: 1:1
Channel No: 0 Name: BCH
CFN: 150

Message Details:

SIB repetition period:64
SIB position:52
SIB size:246
SIB (raw):

[0]00 02 B2 20 D9 0A 00 8C
[8]84 25 25 A6 39 A0 08 8A
[16]64 4C 73 40 02 22 32 55
[24]01 28 52 A1 84 A2 08 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 02 B2 20 D9 0A 00 8C
[8]84 25 25 A6 39 A0 08 8A
[16]64 4C 73 40 02 22 32 55
[24]01 28 52 A1 84 A2 08

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:00:09.110

Channel ID: RbBcch
Cell ID: 0

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:0

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:3
sg_POS:0
bcch_ModificationTime: Omit

#### MAC_DATA_REQ

RLC MAC @ 00:00:09.110

Category: Configuration
BTS unit: 1:1
Channel No: 0 Name: BCCH
CFN: 152

Message Details:

RLC PDU size (bits):56
RLC PDU (raw):

[0]00 0E 07 17 82 80 81

#### MAC_DATA_REQ

RLC MAC @ 00:00:09.110

Category: Configuration
BTS unit: 1:1
Channel No: 0 Name: BCCH
CFN: 152

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]00 06 C1 6F F8 D3 4E 52
[8]5A 63 9A 00 8E 57 0A 63
[16]9A 00

#### MAC_DATA_REQ

RLC MAC @ 00:00:09.110

Category: Configuration
BTS unit: 1:1
Channel No: 0 Name: BCCH
CFN: 152

Message Details:

RLC PDU size (bits):168
RLC PDU (raw):

[0]00 0E 27 17 82 80 81 D3
[8]14 43 80 10 46 00 41 18
[16]01 04 60 08 21

#### MAC_DATA_REQ

RLC MAC @ 00:00:09.110

Category: Configuration
BTS unit: 1:1
Channel No: 0 Name: BCCH
CFN: 152

Message Details:

RLC PDU size (bits):160
RLC PDU (raw):

[0]00 0E 1B 7B 10 A8 82 30
[8]5D 4E 49 A1 01 5B 92 2C
[16]44 32 89 70

#### PHY_DATA_REQ

MAC PHY @ 00:00:09.110

BTS unit: 1:1
Channel No: 0 Name: BCH
CFN: 152

Message Details:

SIB repetition period:64
SIB position:58
SIB size:246
SIB (raw):

[0]00 06 B1 87 80 32 32 F8
[8]D3 4E 52 58 63 9A 00 8E
[16]57 08 63 9A 00 22 32 55
[24]01 28 52 A1 84 A2 08 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 06 B1 87 80 32 32 F8
[8]D3 4E 52 58 63 9A 00 8E
[16]57 08 63 9A 00 22 32 55
[24]01 28 52 A1 84 A2 08

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:00:09.120

Channel ID: RbBcch
Cell ID: 0

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:0

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:00:09.120

Channel ID: RbBcch
Cell ID: 0

Message Details:

RLC_TR_DATA_REQ:

cellId:0

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

completeSIB_List:

CompleteSIBshort:

sib_Type:masterInformationBlock
sib_Data_variable:0000000000000000010000000010010110101010000100010000000000001000100010100000101000100010100001001000100001110001101000100111110010001110010010010010000100000001

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:00:09.120

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 8

SIB position: 0

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

completeSIB_List:

CompleteSIB_List.element:

sib_Type: masterInformationBlock_SIB_Type [enum=0]

sib_Data_variable: 0000000000000000010000000010010110101010000100010000000000001000100010100000101000100010100001001000100001110001101000100111110010001110010010010010000100000001

Layer 3 SDU:

[0]00 0E 00 9F 00 00 40 25
[8]AA 11 00 08 8A 0A 22 84
[16]88 71 A2 7C 8E 49 21 01

#### MAC_DATA_REQ

RLC MAC @ 00:00:09.130

Category: Configuration
BTS unit: 1:1
Channel No: 0 Name: BCCH
CFN: 154

Message Details:

RLC PDU size (bits):192
RLC PDU (raw):

[0]00 0E 00 9F 00 00 40 25
[8]AA 11 00 08 8A 0A 22 84
[16]88 71 A2 7C 8E 49 21 01

#### PHY_DATA_REQ

MAC PHY @ 00:00:09.130

BTS unit: 1:1
Channel No: 0 Name: BCH
CFN: 154

Message Details:

SIB repetition period:64
SIB position:26
SIB size:246
SIB (raw):

[0]00 04 C0 9A A1 84 A9 31
[8]B2 DF D2 EA 53 22 63 9A
[16]00 88 54 B2 63 9A 00 8A
[24]55 7A 63 9A 00 C8 C8 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 04 C0 9A A1 84 A9 31
[8]B2 DF D2 EA 53 22 63 9A
[16]00 88 54 B2 63 9A 00 8A
[24]55 7A 63 9A 00 C8 C8

#### PHY_DATA_REQ

MAC PHY @ 00:00:09.150

BTS unit: 1:1
Channel No: 0 Name: BCH
CFN: 156

Message Details:

SIB repetition period:64
SIB position:22
SIB size:246
SIB (raw):

[0]00 02 C2 01 B2 0C 25 25
[8]A6 39 A0 08 8A 64 4C 73
[16]40 02 22 32 55 01 28 52
[24]01 84 A2 0A 10 C2 50 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 02 C2 01 B2 0C 25 25
[8]A6 39 A0 08 8A 64 4C 73
[16]40 02 22 32 55 01 28 52
[24]01 84 A2 0A 10 C2 50

#### PHY_DATA_REQ

MAC PHY @ 00:00:09.170

BTS unit: 1:1
Channel No: 0 Name: BCH
CFN: 158

Message Details:

SIB repetition period:64
SIB position:30
SIB size:246
SIB (raw):

[0]00 0E 07 17 82 80 81 25
[8]A6 39 A0 08 8A 64 4C 73
[16]40 02 22 32 55 01 28 52
[24]01 84 A2 0A 10 C2 50 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 0E 07 17 82 80 81 25
[8]A6 39 A0 08 8A 64 4C 73
[16]40 02 22 32 55 01 28 52
[24]01 84 A2 0A 10 C2 50

#### PHY_DATA_REQ

MAC PHY @ 00:00:09.190

BTS unit: 1:1
Channel No: 0 Name: BCH
CFN: 160

Message Details:

SIB repetition period:64
SIB position:28
SIB size:246
SIB (raw):

[0]00 06 C1 6F F8 D3 4E 52
[8]5A 63 9A 00 8E 57 0A 63
[16]9A 00 22 32 55 01 28 52
[24]01 84 A2 0A 10 C2 50 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 06 C1 6F F8 D3 4E 52
[8]5A 63 9A 00 8E 57 0A 63
[16]9A 00 22 32 55 01 28 52
[24]01 84 A2 0A 10 C2 50

#### PHY_DATA_REQ

MAC PHY @ 00:00:09.210

BTS unit: 1:1
Channel No: 0 Name: BCH
CFN: 162

Message Details:

SIB repetition period:64
SIB position:46
SIB size:246
SIB (raw):

[0]00 0E 27 17 82 80 81 D3
[8]14 43 80 10 46 00 41 18
[16]01 04 60 08 21 01 28 52
[24]01 84 A2 0A 10 C2 50 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 0E 27 17 82 80 81 D3
[8]14 43 80 10 46 00 41 18
[16]01 04 60 08 21 01 28 52
[24]01 84 A2 0A 10 C2 50

#### PHY_DATA_REQ

MAC PHY @ 00:00:09.230

BTS unit: 1:1
Channel No: 0 Name: BCH
CFN: 164

Message Details:

SIB repetition period:16
SIB position:2
SIB size:246
SIB (raw):

[0]00 0E 1B 7B 10 A8 82 30
[8]5D 4E 49 A1 01 5B 92 2C
[16]44 32 89 70 21 01 28 52
[24]01 84 A2 0A 10 C2 50 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 0E 1B 7B 10 A8 82 30
[8]5D 4E 49 A1 01 5B 92 2C
[16]44 32 89 70 21 01 28 52
[24]01 84 A2 0A 10 C2 50

#### PHY_DATA_REQ

MAC PHY @ 00:00:09.250

BTS unit: 1:1
Channel No: 0 Name: BCH
CFN: 166

Message Details:

SIB repetition period:8
SIB position:0
SIB size:246
SIB (raw):

[0]00 0E 00 9F 00 00 40 25
[8]AA 11 00 08 8A 0A 22 84
[16]88 71 A2 7C 8E 49 21 01
[24]01 84 A2 0A 10 C2 50 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 0E 00 9F 00 00 40 25
[8]AA 11 00 08 8A 0A 22 84
[16]88 71 A2 7C 8E 49 21 01
[24]01 84 A2 0A 10 C2 50

#### CMAC_PAGING_Config_REQ

RRC LLA @ 00:00:14.140

Channel ID: S-CCPCH#1
Cell ID: 0

Message Details:

CMAC_PAGING_Config_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:5

ratType:fdd

configMessage: (CmacPagingConfigReq)

pI_BitMapInfo:

e18:000000000000000100

dRX_CycleLength:7

iMSI: (IMSI_GSM_MAP)

Digit:0
Digit:0
Digit:1
Digit:0
Digit:1
Digit:0
Digit:0
Digit:0
Digit:0
Digit:0
Digit:0
Digit:0
Digit:3
Digit:3
Digit:3

t_pich_T_sccpch:false

#### CMAC_PAGING_Config_CNF

LLA RRC @ 00:00:14.150

Channel ID: S-CCPCH#1
Cell ID: 0

Message Details:

CMAC_PAGING_Config_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:5

#### RLC_TR_DATA_REQ

RRC LLA @ 00:00:14.150

Channel ID: RbPcch
Cell ID: 0

Message Details:

RLC_TR_DATA_REQ:

cellId:0

routingInfo:

rB_Identity:-2

tM_message:

pCCH_Message:

message: (PCCH_MessageType)

pagingType1:

pagingRecordList: Omit

bcch_ModificationInfo:

mib_ValueTag:1
bcch_ModificationTime: Omit

laterNonCriticalExtensions: Omit

#### RLC_TR_DATA_REQ: pagingType1

LLA RLC @ 00:00:14.150

Channel No: 0 Name: PCCH

Message Details:

Paging Indicator: 15

DRX Cycle Length: 128

Paging Occasion: 77

PCCH_Message:

message:

pagingType1:

pagingRecordList: Omitted

bcch_ModificationInfo:

mib_ValueTag: 1

bcch_ModificationTime: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]20

#### RLC_TR_DATA_REQ

RRC LLA @ 00:00:14.150

Channel ID: RbBcchFach
Cell ID: 0

Message Details:

RLC_TR_DATA_REQ:

cellId:0

routingInfo:

rB_Identity:-3

tM_message:

bCCH_FACH_Message:

message: (BCCH_FACH_MessageType)

systemInformationChangeIndication:

bcch_ModificationInfo:

mib_ValueTag:1
bcch_ModificationTime: Omit

laterNonCriticalExtensions: Omit

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:00:14.150

Channel No: 1 Name: BCCH

Message Details:

SIB repetition rate: 8

SIB position: 0

BCCH_FACH_Message:

message:

systemInformationChangeIndication:

bcch_ModificationInfo:

mib_ValueTag: 1

bcch_ModificationTime: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]40

#### MMI_CmdReq

RRC LLA @ 00:00:14.150

Message Details:

MMI_CmdReq:

cmd (IA5String):Please switch on the UE

#### CMAC Configuration REQ

LLA MAC @ 00:00:14.170

BTS unit: 1:1
Channel No: 0 Name: S_CCPCH
CFN: 146

Message Details:

Configuration Parameters:

Number Of Transport Channels:3

Transport Channels:

Item Number 0:

Transport Channel Parameters:

Transport Channel:

Name:PCH
Identity:0

TTI (ms):10
EP Type:1/2 Rate Convolutional Coding
CRC Size:16
RM Attribute:230
First Interleave:On
Number Of Transport Formats:2

Transport Format Set:

Transport Format 0:

Number Of Transport Blocks:0
Transport Block Size In Bits:240

Transport Format 1:

Number Of Transport Blocks:1
Transport Block Size In Bits:240

Number Of Logical Channels:1

Logical Channels:

Item Number 0:

Logical Channel:

Name:PCCH
Identity:0

Priority:1
CT Length:0
CT Value:0
TCTF Length:0
TCTF Value:0
UE ID Type:Not used
UE ID:0

Item Number 1:

Transport Channel Parameters:

Transport Channel:

Name:FACH
Identity:0

TTI (ms):10
EP Type:1/2 Rate Convolutional Coding
CRC Size:16
RM Attribute:220
First Interleave:On
Number Of Transport Formats:3

Transport Format Set:

Transport Format 0:

Number Of Transport Blocks:0
Transport Block Size In Bits:168

Transport Format 1:

Number Of Transport Blocks:1
Transport Block Size In Bits:168

Transport Format 2:

Number Of Transport Blocks:2
Transport Block Size In Bits:168

Number Of Logical Channels:6

Logical Channels:

Item Number 0:

Logical Channel:

Name:BCCH
Identity:1

Priority:6
CT Length:0
CT Value:0
TCTF Length:2
TCTF Value:0
UE ID Type:Not used
UE ID:0

Item Number 1:

Logical Channel:

Name:CCCH
Identity:1

Priority:1
CT Length:0
CT Value:0
TCTF Length:8
TCTF Value:64
UE ID Type:Not used
UE ID:0

Item Number 2:

Logical Channel:

Name:DCCH
Identity:1

Priority:1
CT Length:4
CT Value:0
TCTF Length:2
TCTF Value:3
UE ID Type:C RNTI
UE ID:1

Item Number 3:

Logical Channel:

Name:DCCH
Identity:2

Priority:2
CT Length:4
CT Value:1
TCTF Length:2
TCTF Value:3
UE ID Type:C RNTI
UE ID:1

Item Number 4:

Logical Channel:

Name:DCCH
Identity:3

Priority:3
CT Length:4
CT Value:2
TCTF Length:2
TCTF Value:3
UE ID Type:C RNTI
UE ID:1

Item Number 5:

Logical Channel:

Name:DCCH
Identity:4

Priority:4
CT Length:4
CT Value:3
TCTF Length:2
TCTF Value:3
UE ID Type:C RNTI
UE ID:1

Item Number 2:

Transport Channel Parameters:

Transport Channel:

Name:FACH
Identity:1

TTI (ms):10
EP Type:Turbo Coding
CRC Size:16
RM Attribute:130
First Interleave:On
Number Of Transport Formats:2

Transport Format Set:

Transport Format 0:

Number Of Transport Blocks:0
Transport Block Size In Bits:360

Transport Format 1:

Number Of Transport Blocks:1
Transport Block Size In Bits:360

Number Of Logical Channels:1

Logical Channels:

Item Number 0:

Logical Channel:

Name:D_DTCH
Identity:4

Priority:8
CT Length:4
CT Value:6
TCTF Length:2
TCTF Value:3
UE ID Type:C RNTI
UE ID:1

Active Flag:1

Transport Format Combination Set:

Number Of Transport Format Combinations:8

Transport Format Combinations 0:

Transport Format:0
Transport Format:0
Transport Format:0

Transport Format Combinations 1:

Transport Format:1
Transport Format:0
Transport Format:0

Transport Format Combinations 2:

Transport Format:0
Transport Format:1
Transport Format:0

Transport Format Combinations 3:

Transport Format:1
Transport Format:1
Transport Format:0

Transport Format Combinations 4:

Transport Format:0
Transport Format:2
Transport Format:0

Transport Format Combinations 5:

Transport Format:1
Transport Format:2
Transport Format:0

Transport Format Combinations 6:

Transport Format:0
Transport Format:0
Transport Format:1

Transport Format Combinations 7:

Transport Format:0
Transport Format:1
Transport Format:1

#### CMAC Configuration CNF

MAC LLA @ 00:00:14.170

BTS unit: 1:1
Channel No: 0 Name: S_CCPCH
CFN: 146

Message Details:

#### MAC_DATA_REQ

RLC MAC @ 00:00:14.180

Category: Configuration
BTS unit: 1:1
Channel No: 0 Name: PCCH
CFN: 147

Message Details:

RLC PDU size (bits):8
RLC PDU (raw):

[0]20

#### MAC_DATA_REQ

RLC MAC @ 00:00:14.180

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: BCCH
CFN: 147

Message Details:

RLC PDU size (bits):8
RLC PDU (raw):

[0]40

#### PHY_DATA_REQ

MAC PHY @ 00:00:14.180

BTS unit: 1:1
Channel No: 0 Name: FACH
CFN: 147

Message Details:

TFI:1
TB set size:168
TB size:168
TB set (raw):

[0]10 00 00 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00 00 00

TB set (decoded):

TB 0:

TCTF:0
MAC SDU (166 bits):

[0]40 00 00 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00 00

#### PHY_DATA_REQ

MAC PHY @ 00:00:14.780

BTS unit: 1:1
Channel No: 0 Name: PCH
CFN: 207

Message Details:

TFI:1
TB set size:240
TB size:240
TB set (raw):

[0]20 00 00 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00 00 00 00 00
[24]00 00 00 00 00 00

TB set (decoded):

TB 0:

MAC SDU (240 bits):

[0]20 00 00 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00 00 00 00 00
[24]00 00 00 00 00 00

#### MMI_CmdCnf

LLA RRC @ 00:00:16.540

Message Details:

MMI_CmdCnf:

result:true
resultString (IA5String): Omit

#### MMI_CmdReq

RRC LLA @ 00:00:16.540

Message Details:

MMI_CmdReq:

cmd (IA5String):Please switch on the UE

#### MMI_CmdCnf

LLA RRC @ 00:00:18.010

Message Details:

MMI_CmdCnf:

result:true
resultString (IA5String): Omit

#### PHY_DATA_IND

PHY MAC @ 00:01:03.610

BTS unit: 1:1
Channel No: 0 Name: U_RACH
CFN: 206

Message Details:

TFI:0
TB set size:168
TB size:168
TB set (raw):

[0]08 44 48 8C D1 00 10 42
[8]00 02 C0 00 00 00 00 00
[16]00 00 00 00 00 00

TB set (decoded):

TB 0:

TCTF:0
MAC SDU (166 bits):

[0]21 11 22 33 44 00 41 08
[8]00 0B 00 00 00 00 00 00
[16]00 00 00 00 00

#### MAC_DATA_IND

MAC RLC @ 00:01:03.610

Category: Configuration
BTS unit: 1:1
Channel No: 0 Name: CCCH
CFN: 206

Message Details:

RLC PDU size (bits):166
RLC PDU (raw):

[0]21 11 22 33 44 00 41 08
[8]00 0B 00 00 00 00 00 00
[16]00 00 00 00 00

#### RLC_TR_DATA_IND: rrcConnectionRequest

RLC LLA @ 00:01:03.620

Channel No: 0 Name: CCCH

Message Details:

UL_CCCH_Message:

integrityCheckInfo: Omitted

message:

rrcConnectionRequest:

initialUE_Identity:

tmsi_and_LAI:

tmsi: 00010001001000100011001101000100

lai:

plmn_Identity:

mcc:

MCC.element: 0

MCC.element: 0

MCC.element: 4

mnc:

MNC.element: 2

MNC.element: 1

lac: 0000000000000001

establishmentCause: registration_EstablishmentCause [enum=12]

protocolErrorIndicator: noError_ProtocolErrorIndicator [enum=0]

measuredResultsOnRACH: Omitted

v3d0NonCriticalExtensions: Omitted

Layer 3 SDU:

[0]21 11 22 33 44 00 41 08
[8]00 0B 00 00 00 00 00 00
[16]00 00 00 00 00

#### RLC_TR_DATA_IND

LLA RRC @ 00:01:03.620

Channel ID: Rb0
Cell ID: 0

Message Details:

RLC_TR_DATA_IND:

cellId:0

routingInfo:

rB_Identity:0

tM_message:

uL_CCCH_Message:

integrityCheckInfo: Omit

message: (UL_CCCH_MessageType)

rrcConnectionRequest:

initialUE_Identity:

tmsi_and_LAI: (TMSI_and_LAI_GSM_MAP)

tmsi (TMSI_GSM_MAP):00010001001000100011001101000100

lai:

plmn_Identity:

mcc:

Digit:0
Digit:0
Digit:4

mnc:

Digit:2
Digit:1

lac:0000000000000001

establishmentCause:registration
protocolErrorIndicator:noError

measuredResultsOnRACH: Omit

v3d0NonCriticalExtensions: Omit

#### RLC_UM_DATA_REQ

RRC LLA @ 00:01:03.620

Channel ID: Rb0
Cell ID: 0

Message Details:

RLC_UM_DATA_REQ:

cellId:0

routingInfo:

rB_Identity:0

uM_message:

dL_CCCH_Message:

integrityCheckInfo: Omit

message: (DL_CCCH_MessageType)

rrcConnectionSetup:

r3:

rrcConnectionSetup_r3: (RRCConnectionSetup_r3_IEs)

initialUE_Identity:

tmsi_and_LAI: (TMSI_and_LAI_GSM_MAP)

tmsi (TMSI_GSM_MAP):00010001001000100011001101000100

lai:

plmn_Identity:

mcc:

Digit:0
Digit:0
Digit:4

mnc:

Digit:2
Digit:1

lac:0000000000000001

rrc_TransactionIdentifier:0
activationTime: Omit

new_U_RNTI: (U_RNTI)

srnc_Identity:000000000001
s_RNTI:00000000000000000001

new_c_RNTI (C_RNTI):0000000000000001
rrc_StateIndicator:cell_FACH
utran_DRX_CycleLengthCoeff (UTRAN_DRX_CycleLengthCoefficient):9

capabilityUpdateRequirement:

ue_RadioCapabilityFDDUpdateRequirement:true
ue_RadioCapabilityTDDUpdateRequirement:false

systemSpecificCapUpdateReqList:

SystemSpecificCapUpdateReq:gsm

srb_InformationSetupList: (SRB_InformationSetupList2)

SRB_InformationSetup:

rb_Identity:1

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_UM_RLC_Mode:

transmissionRLC_Discard:

timerBasedNoExplicit (NoExplicitDiscard):dt50

dl_RLC_Mode:

dl_UM_RLC_Mode:

rb_MappingInfo:

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

rach:

logicalChannelIdentity:1

rlc_SizeList:

explicitList: (RLC_SizeExplicitList)

RLC_SizeInfo:

rlc_SizeIndex:1

mac_LogicalChannelPriority:1

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

fach:

logicalChannelIdentity:1

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

dch (TransportChannelIdentity):5

logicalChannelIdentity:1

rlc_SizeList:

configured:

mac_LogicalChannelPriority:1

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

dch (TransportChannelIdentity):10

logicalChannelIdentity:1

SRB_InformationSetup:

rb_Identity:2

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp400
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

rb_MappingInfo:

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

rach:

logicalChannelIdentity:2

rlc_SizeList:

explicitList: (RLC_SizeExplicitList)

RLC_SizeInfo:

rlc_SizeIndex:1

mac_LogicalChannelPriority:2

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

fach:

logicalChannelIdentity:2

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

dch (TransportChannelIdentity):5

logicalChannelIdentity:2

rlc_SizeList:

configured:

mac_LogicalChannelPriority:2

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

dch (TransportChannelIdentity):10

logicalChannelIdentity:2

SRB_InformationSetup:

rb_Identity:3

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp400
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

rb_MappingInfo:

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

rach:

logicalChannelIdentity:3

rlc_SizeList:

explicitList: (RLC_SizeExplicitList)

RLC_SizeInfo:

rlc_SizeIndex:1

mac_LogicalChannelPriority:3

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

fach:

logicalChannelIdentity:3

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

dch (TransportChannelIdentity):5

logicalChannelIdentity:3

rlc_SizeList:

configured:

mac_LogicalChannelPriority:3

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

dch (TransportChannelIdentity):10

logicalChannelIdentity:3

SRB_InformationSetup:

rb_Identity:4

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp400
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

rb_MappingInfo:

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

rach:

logicalChannelIdentity:4

rlc_SizeList:

explicitList: (RLC_SizeExplicitList)

RLC_SizeInfo:

rlc_SizeIndex:1

mac_LogicalChannelPriority:4

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

fach:

logicalChannelIdentity:4

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

dch (TransportChannelIdentity):5

logicalChannelIdentity:4

rlc_SizeList:

configured:

mac_LogicalChannelPriority:4

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

dch (TransportChannelIdentity):10

logicalChannelIdentity:4

ul_CommonTransChInfo:

tfc_Subset: Omit

prach_TFCS: (TFCS) Omit

modeSpecificInfo:

fdd:

ul_TFCS: (TFCS)

normalTFCI_Signalling: (ExplicitTFCS_Configuration)

complete: (TFCS_ReconfAdd)

ctfcSize:

ctfc2Bit:

:

ctfc2:0

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc2:1

powerOffsetInformation:

gainFactorInformation:

signalledGainFactors:

modeSpecificInfo:

fdd:

gainFactorBetaC (GainFactor):11

gainFactorBetaD (GainFactor):15
referenceTFC_ID:0

powerOffsetPp_m: Omit

ul_AddReconfTransChInfoList:

UL_AddReconfTransChInformation:

ul_TransportChannelType (UL_TrCH_Type):dch
transportChannelIdentity:5

transportFormatSet:

dedicatedTransChTFS:

tti:

tti40: (DedicatedDynamicTF_InfoList)

DedicatedDynamicTF_Info:

rlc_Size:

bitMode: (BitModeRLC_SizeInfo)

sizeType2:

part1:2
part2: Omit

numberOfTbSizeList:

NumberOfTransportBlocks:

zero:

NumberOfTransportBlocks:

one:

logicalChannelList:

allSizes:

semistaticTF_Information:

channelCodingType:

convolutional (CodingRate):third

rateMatchingAttribute:170
crc_Size:crc16

dl_CommonTransChInfo:

sccpch_TFCS: (TFCS) Omit

modeSpecificInfo:

fdd:

dl_Parameters:

sameAsUL:

dl_AddReconfTransChInfoList:

DL_AddReconfTransChInformation:

dl_TransportChannelType (DL_TrCH_Type):dch
dl_transportChannelIdentity (TransportChannelIdentity):10

tfs_SignallingMode:

sameAsULTrCH: (UL_TransportChannelIdentity)

ul_TransportChannelType (UL_TrCH_Type):dch
ul_TransportChannelIdentity (TransportChannelIdentity):5

dch_QualityTarget: (QualityTarget)

bler_QualityValue:-20

dummy: (TM_SignallingInfo) Omit

frequencyInfo: Omit

maxAllowedUL_TX_Power: Omit

ul_ChannelRequirement: Omit

dl_CommonInformation: Omit

dl_InformationPerRL_List: Omit

laterNonCriticalExtensions: Omit

specialLI:true

#### RLC_UM_DATA_REQ: rrcConnectionSetup

LLA RLC @ 00:01:03.620

Channel No: 1 Name: CCCH

Message Details:

DL_CCCH_Message:

integrityCheckInfo: Omitted

message:

rrcConnectionSetup:

r3:

rrcConnectionSetup_r3:

initialUE_Identity:

tmsi_and_LAI:

tmsi: 00010001001000100011001101000100

lai:

plmn_Identity:

mcc:

MCC.element: 0

MCC.element: 0

MCC.element: 4

mnc:

MNC.element: 2

MNC.element: 1

lac: 0000000000000001

rrc_TransactionIdentifier: 0

activationTime: Omitted

new_U_RNTI:

srnc_Identity: 000000000001

s_RNTI: 00000000000000000001

new_c_RNTI: 0000000000000001

rrc_StateIndicator: cell_FACH_RRC_StateIndicator [enum=1]

utran_DRX_CycleLengthCoeff: 9

capabilityUpdateRequirement:

ue_RadioCapabilityFDDUpdateRequirement: 1

ue_RadioCapabilityTDDUpdateRequirement: 0

systemSpecificCapUpdateReqList:

SystemSpecificCapUpdateReqList.element: gsm_SystemSpecificCapUpdateReq [enum=0]

srb_InformationSetupList:

SRB_InformationSetupList2.element:

rb_Identity: 1

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_UM_RLC_Mode:

transmissionRLC_Discard:

timerBasedNoExplicit: dt50_NoExplicitDiscard [enum=4]

dl_RLC_Mode:

dl_UM_RLC_Mode: NULL

rb_MappingInfo:

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

rach: NULL

logicalChannelIdentity: 1

rlc_SizeList:

explicitList:

RLC_SizeExplicitList.element:

rlc_SizeIndex: 1

mac_LogicalChannelPriority: 1

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

fach: NULL

logicalChannelIdentity: 1

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

dch: 5

logicalChannelIdentity: 1

rlc_SizeList:

configured: NULL

mac_LogicalChannelPriority: 1

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

dch: 10

logicalChannelIdentity: 1

SRB_InformationSetupList2.element:

rb_Identity: 2

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard: dat15_MaxDAT [enum=10]

transmissionWindowSize: tw32_TransmissionWindowSize [enum=3]

timerRST: tr500_TimerRST [enum=9]

max_RST: rst1_MaxRST [enum=0]

pollingInfo:

timerPollProhibit: tpp200_TimerPollProhibit [enum=19]

timerPoll: tp400_TimerPoll [enum=39]

poll_PDU: Omitted

poll_SDU: sdu1_Poll_SDU [enum=0]

lastTransmissionPDU_Poll: 1

lastRetransmissionPDU_Poll: 1

pollWindow: pw99_PollWindow [enum=7]

timerPollPeriodic: Omitted

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery: 1

receivingWindowSize: rw32_ReceivingWindowSize [enum=3]

dl_RLC_StatusInfo:

timerStatusProhibit: tsp200_TimerStatusProhibit [enum=19]

timerEPC: Omitted

missingPDU_Indicator: 1

timerStatusPeriodic: Omitted

rb_MappingInfo:

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

rach: NULL

logicalChannelIdentity: 2

rlc_SizeList:

explicitList:

RLC_SizeExplicitList.element:

rlc_SizeIndex: 1

mac_LogicalChannelPriority: 2

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

fach: NULL

logicalChannelIdentity: 2

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

dch: 5

logicalChannelIdentity: 2

rlc_SizeList:

configured: NULL

mac_LogicalChannelPriority: 2

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

dch: 10

logicalChannelIdentity: 2

SRB_InformationSetupList2.element:

rb_Identity: 3

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard: dat15_MaxDAT [enum=10]

transmissionWindowSize: tw32_TransmissionWindowSize [enum=3]

timerRST: tr500_TimerRST [enum=9]

max_RST: rst1_MaxRST [enum=0]

pollingInfo:

timerPollProhibit: tpp200_TimerPollProhibit [enum=19]

timerPoll: tp400_TimerPoll [enum=39]

poll_PDU: Omitted

poll_SDU: sdu1_Poll_SDU [enum=0]

lastTransmissionPDU_Poll: 1

lastRetransmissionPDU_Poll: 1

pollWindow: pw99_PollWindow [enum=7]

timerPollPeriodic: Omitted

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery: 1

receivingWindowSize: rw32_ReceivingWindowSize [enum=3]

dl_RLC_StatusInfo:

timerStatusProhibit: tsp200_TimerStatusProhibit [enum=19]

timerEPC: Omitted

missingPDU_Indicator: 1

timerStatusPeriodic: Omitted

rb_MappingInfo:

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

rach: NULL

logicalChannelIdentity: 3

rlc_SizeList:

explicitList:

RLC_SizeExplicitList.element:

rlc_SizeIndex: 1

mac_LogicalChannelPriority: 3

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

fach: NULL

logicalChannelIdentity: 3

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

dch: 5

logicalChannelIdentity: 3

rlc_SizeList:

configured: NULL

mac_LogicalChannelPriority: 3

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

dch: 10

logicalChannelIdentity: 3

SRB_InformationSetupList2.element:

rb_Identity: 4

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard: dat15_MaxDAT [enum=10]

transmissionWindowSize: tw32_TransmissionWindowSize [enum=3]

timerRST: tr500_TimerRST [enum=9]

max_RST: rst1_MaxRST [enum=0]

pollingInfo:

timerPollProhibit: tpp200_TimerPollProhibit [enum=19]

timerPoll: tp400_TimerPoll [enum=39]

poll_PDU: Omitted

poll_SDU: sdu1_Poll_SDU [enum=0]

lastTransmissionPDU_Poll: 1

lastRetransmissionPDU_Poll: 1

pollWindow: pw99_PollWindow [enum=7]

timerPollPeriodic: Omitted

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery: 1

receivingWindowSize: rw32_ReceivingWindowSize [enum=3]

dl_RLC_StatusInfo:

timerStatusProhibit: tsp200_TimerStatusProhibit [enum=19]

timerEPC: Omitted

missingPDU_Indicator: 1

timerStatusPeriodic: Omitted

rb_MappingInfo:

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

rach: NULL

logicalChannelIdentity: 4

rlc_SizeList:

explicitList:

RLC_SizeExplicitList.element:

rlc_SizeIndex: 1

mac_LogicalChannelPriority: 4

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

fach: NULL

logicalChannelIdentity: 4

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

dch: 5

logicalChannelIdentity: 4

rlc_SizeList:

configured: NULL

mac_LogicalChannelPriority: 4

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

dch: 10

logicalChannelIdentity: 4

ul_CommonTransChInfo:

tfc_Subset: Omitted

prach_TFCS: Omitted

modeSpecificInfo:

fdd:

ul_TFCS:

normalTFCI_Signalling:

complete:

ctfcSize:

ctfc2Bit:

ctfc2Bit.noName:

ctfc2: 0

powerOffsetInformation:

gainFactorInformation:

computedGainFactors: 0

powerOffsetPp_m: Omitted

ctfc2Bit.noName:

ctfc2: 1

powerOffsetInformation:

gainFactorInformation:

signalledGainFactors:

modeSpecificInfo:

fdd:

gainFactorBetaC: 11

gainFactorBetaD: 15

referenceTFC_ID: 0

powerOffsetPp_m: Omitted

ul_AddReconfTransChInfoList:

UL_AddReconfTransChInfoList.element:

ul_TransportChannelType: dch_UL_TrCH_Type [enum=0]

transportChannelIdentity: 5

transportFormatSet:

dedicatedTransChTFS:

tti:

tti40:

DedicatedDynamicTF_InfoList.element:

rlc_Size:

bitMode:

sizeType2:

part1: 2

part2: Omitted

numberOfTbSizeList:

numberOfTbSizeList.element:

zero: NULL

numberOfTbSizeList.element:

one: NULL

logicalChannelList:

allSizes: NULL

semistaticTF_Information:

channelCodingType:

convolutional: third_CodingRate [enum=1]

rateMatchingAttribute: 170

crc_Size: crc16_CRC_Size [enum=3]

dl_CommonTransChInfo:

sccpch_TFCS: Omitted

modeSpecificInfo:

fdd:

dl_Parameters:

sameAsUL: NULL

dl_AddReconfTransChInfoList:

DL_AddReconfTransChInfoList.element:

dl_TransportChannelType: dch_DL_TrCH_Type [enum=0]

dl_transportChannelIdentity: 10

tfs_SignallingMode:

sameAsULTrCH:

ul_TransportChannelType: dch_UL_TrCH_Type [enum=0]

ul_TransportChannelIdentity: 5

dch_QualityTarget:

bler_QualityValue: -20

dummy: Omitted

frequencyInfo: Omitted

maxAllowedUL_TX_Power: Omitted

ul_ChannelRequirement: Omitted

dl_CommonInformation: Omitted

dl_InformationPerRL_List: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]31 E0 22 24 46 68 80 08
[8]21 00 01 00 04 00 00 40
[16]00 5D 83 03 6A 27 50 80
[24]00 A1 A1 01 08 90 85 9E
[32]8E 46 C9 CE 7C 9C 4E 75
[40]18 00 2A 3A 10 52 89 18
[48]99 E8 E4 6C 9C E7 C9 C4
[56]E7 52 80 04 A5 A1 09 48
[64]92 8D 9E 8E 46 C9 CE 7C
[72]9C 4E 75 38 00 6A 7A 10
[80]D6 89 32 00 01 89 4A FC
[88]00 84 02 20 88 EA 59 82
[96]26 25 60

#### MAC_DATA_REQ

RLC MAC @ 00:01:03.660

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: CCCH
CFN: 231

Message Details:

RLC PDU size (bits):160
RLC PDU (raw):

[0]01 F8 31 E0 22 24 46 68
[8]80 08 21 00 01 00 04 00
[16]00 40 00 5D

RLC PDU (decoded):

Sequence number:0
Length indicator 0 (octets):124 (the first data octet in this RLC PDU is the first octet of a RLC SDU)
Segment associated with length indicator 0 (0 octets):

Last segment, not associated with any length indicators (18 octets):

[0]31 E0 22 24 46 68 80 08
[8]21 00 01 00 04 00 00 40
[16]00 5D

#### MAC_DATA_REQ

RLC MAC @ 00:01:03.660

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: CCCH
CFN: 231

Message Details:

RLC PDU size (bits):160
RLC PDU (raw):

[0]02 83 03 6A 27 50 80 00
[8]A1 A1 01 08 90 85 9E 8E
[16]46 C9 CE 7C

RLC PDU (decoded):

Sequence number:1
Last segment, not associated with any length indicators (19 octets):

[0]83 03 6A 27 50 80 00 A1
[8]A1 01 08 90 85 9E 8E 46
[16]C9 CE 7C

#### MAC_DATA_REQ

RLC MAC @ 00:01:03.660

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: CCCH
CFN: 231

Message Details:

RLC PDU size (bits):160
RLC PDU (raw):

[0]04 9C 4E 75 18 00 2A 3A
[8]10 52 89 18 99 E8 E4 6C
[16]9C E7 C9 C4

RLC PDU (decoded):

Sequence number:2
Last segment, not associated with any length indicators (19 octets):

[0]9C 4E 75 18 00 2A 3A 10
[8]52 89 18 99 E8 E4 6C 9C
[16]E7 C9 C4

#### MAC_DATA_REQ

RLC MAC @ 00:01:03.660

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: CCCH
CFN: 231

Message Details:

RLC PDU size (bits):160
RLC PDU (raw):

[0]06 E7 52 80 04 A5 A1 09
[8]48 92 8D 9E 8E 46 C9 CE
[16]7C 9C 4E 75

RLC PDU (decoded):

Sequence number:3
Last segment, not associated with any length indicators (19 octets):

[0]E7 52 80 04 A5 A1 09 48
[8]92 8D 9E 8E 46 C9 CE 7C
[16]9C 4E 75

#### MAC_DATA_REQ

RLC MAC @ 00:01:03.660

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: CCCH
CFN: 231

Message Details:

RLC PDU size (bits):160
RLC PDU (raw):

[0]08 38 00 6A 7A 10 D6 89
[8]32 00 01 89 4A FC 00 84
[16]02 20 88 EA

RLC PDU (decoded):

Sequence number:4
Last segment, not associated with any length indicators (19 octets):

[0]38 00 6A 7A 10 D6 89 32
[8]00 01 89 4A FC 00 84 02
[16]20 88 EA

#### MAC_DATA_REQ

RLC MAC @ 00:01:03.660

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: CCCH
CFN: 231

Message Details:

RLC PDU size (bits):160
RLC PDU (raw):

[0]0B 0B FE 59 82 26 25 60
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

RLC PDU (decoded):

Sequence number:5
Length indicator 0 (octets):5
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (5 octets):

[0]59 82 26 25 60
Padding associated with length indicator 1 (12 octets):

[0]00 00 00 00 00 00 00 00
[8]00 00 00 00

#### PHY_DATA_REQ

MAC PHY @ 00:01:03.660

BTS unit: 1:1
Channel No: 0 Name: FACH
CFN: 231

Message Details:

TFI:2
TB set size:336
TB size:168
TB set (raw, each TB word aligned):

[0]40 01 F8 31 E0 22 24 46
[8]68 80 08 21 00 01 00 04
[16]00 00 40 00 5D 00 40 02
[24]83 03 6A 27 50 80 00 A1
[32]A1 01 08 90 85 9E 8E 46
[40]C9 CE 7C 00

TB set (decoded):

TB 0:

TCTF:64
MAC SDU (160 bits):

[0]01 F8 31 E0 22 24 46 68
[8]80 08 21 00 01 00 04 00
[16]00 40 00 5D

TB 1:

TCTF:64
MAC SDU (160 bits):

[0]02 83 03 6A 27 50 80 00
[8]A1 A1 01 08 90 85 9E 8E
[16]46 C9 CE 7C

#### PHY_DATA_REQ

MAC PHY @ 00:01:03.670

BTS unit: 1:1
Channel No: 0 Name: FACH
CFN: 232

Message Details:

TFI:2
TB set size:336
TB size:168
TB set (raw, each TB word aligned):

[0]40 04 9C 4E 75 18 00 2A
[8]3A 10 52 89 18 99 E8 E4
[16]6C 9C E7 C9 C4 00 40 06
[24]E7 52 80 04 A5 A1 09 48
[32]92 8D 9E 8E 46 C9 CE 7C
[40]9C 4E 75 00

TB set (decoded):

TB 0:

TCTF:64
MAC SDU (160 bits):

[0]04 9C 4E 75 18 00 2A 3A
[8]10 52 89 18 99 E8 E4 6C
[16]9C E7 C9 C4

TB 1:

TCTF:64
MAC SDU (160 bits):

[0]06 E7 52 80 04 A5 A1 09
[8]48 92 8D 9E 8E 46 C9 CE
[16]7C 9C 4E 75

#### PHY_DATA_REQ

MAC PHY @ 00:01:03.680

BTS unit: 1:1
Channel No: 0 Name: FACH
CFN: 233

Message Details:

TFI:2
TB set size:336
TB size:168
TB set (raw, each TB word aligned):

[0]40 08 38 00 6A 7A 10 D6
[8]89 32 00 01 89 4A FC 00
[16]84 02 20 88 EA 00 40 0B
[24]0B FE 59 82 26 25 60 00
[32]00 00 00 00 00 00 00 00
[40]00 00 00 00

TB set (decoded):

TB 0:

TCTF:64
MAC SDU (160 bits):

[0]08 38 00 6A 7A 10 D6 89
[8]32 00 01 89 4A FC 00 84
[16]02 20 88 EA

TB 1:

TCTF:64
MAC SDU (160 bits):

[0]0B 0B FE 59 82 26 25 60
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

#### PHY_DATA_IND

PHY MAC @ 00:01:03.980

BTS unit: 1:1
Channel No: 0 Name: U_RACH
CFN: 243

Message Details:

TFI:0
TB set size:168
TB size:168
TB set (raw):

[0]50 00 11 80 00 4A 0C 00
[8]00 80 00 05 E2 34 1A 20
[16]90 98 CD 08 C5 00

TB set (decoded):

TB 0:

TCTF:1
UEID type:C-RNTI
UEID:1
C/T:1
MAC SDU (144 bits):

[0]80 00 4A 0C 00 00 80 00
[8]05 E2 34 1A 20 90 98 CD
[16]08 C5

#### MAC_DATA_IND

MAC RLC @ 00:01:03.980

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 243

Message Details:

RLC PDU size (bits):142
RLC PDU (raw):

[0]80 00 4A 0C 00 00 80 00
[8]05 E2 34 1A 20 90 98 CD
[16]08 C5

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:0
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]4A 0C 00 00 80 00 05 E2
[8]34 1A 20 90 98 CD 08 C5

#### PHY_DATA_IND

PHY MAC @ 00:01:04.050

BTS unit: 1:1
Channel No: 0 Name: U_RACH
CFN: 250

Message Details:

TFI:0
TB set size:168
TB size:168
TB set (raw):

[0]50 00 11 80 0D 15 FE 92
[8]60 41 00 01 00 02 31 F1
[16]F0 55 55 55 55 00

TB set (decoded):

TB 0:

TCTF:1
UEID type:C-RNTI
UEID:1
C/T:1
MAC SDU (144 bits):

[0]80 0D 15 FE 92 60 41 00
[8]01 00 02 31 F1 F0 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:01:04.050

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 250

Message Details:

RLC PDU size (bits):142
RLC PDU (raw):

[0]80 0D 15 FE 92 60 41 00
[8]01 00 02 31 F1 F0 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:1
Polling bit:1 (request a status report)
Length indicator 0 (octets):10
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (10 octets):

[0]92 60 41 00 01 00 02 31
[8]F1 F0
Padding associated with length indicator 1 (4 octets):

[0]55 55 55 55

#### RLC_AM_DATA_IND: rrcConnectionSetupComplete

RLC LLA @ 00:01:04.060

Channel No: 2 Name: DCCH

Message Details:

UL_DCCH_Message:

integrityCheckInfo: Omitted

message:

rrcConnectionSetupComplete:

rrc_TransactionIdentifier: 0

startList:

STARTList.element:

cn_DomainIdentity: ps_domain_CN_DomainIdentity [enum=1]

start_Value: 00000000000000000010

STARTList.element:

cn_DomainIdentity: cs_domain_CN_DomainIdentity [enum=0]

start_Value: 00000000000000000010

ue_RadioAccessCapability:

accessStratumReleaseIndicator: r99_AccessStratumReleaseIndicator [enum=0]

pdcp_Capability:

losslessSRNS_RelocationSupport: 1

supportForRfc2507:

supported: by8192_MaxHcContextSpace [enum=4]

rlc_Capability:

totalRLC_AM_BufferSize: kb50_TotalRLC_AM_BufferSize [enum=2]

maximumRLC_WindowSize: mws2047_MaximumRLC_WindowSize [enum=0]

maximumAM_EntityNumber: am6_MaximumAM_EntityNumberRLC_Cap [enum=3]

transportChannelCapability:

dl_TransChCapability:

maxNoBitsReceived: b5120_MaxNoBits [enum=4]

maxConvCodeBitsReceived: b1280_MaxNoBits [enum=1]

turboDecodingSupport:

supported: b5120_MaxNoBits [enum=4]

maxSimultaneousTransChs: e8_MaxSimultaneousTransChsDL [enum=1]

maxSimultaneousCCTrCH_Count: 1

maxReceivedTransportBlocks: tb16_MaxTransportBlocksDL [enum=2]

maxNumberOfTFC: tfc96_MaxNumberOfTFC_DL [enum=4]

maxNumberOfTF: tf64_MaxNumberOfTF [enum=1]

ul_TransChCapability:

maxNoBitsTransmitted: b3840_MaxNoBits [enum=3]

maxConvCodeBitsTransmitted: b1280_MaxNoBits [enum=1]

turboEncodingSupport:

supported: b3840_MaxNoBits [enum=3]

maxSimultaneousTransChs: e8_MaxSimultaneousTransChsUL [enum=2]

modeSpecificInfo:

fdd: NULL

maxTransmittedBlocks: tb8_MaxTransportBlocksUL [enum=2]

maxNumberOfTFC: tfc32_MaxNumberOfTFC_UL [enum=3]

maxNumberOfTF: tf32_MaxNumberOfTF [enum=0]

rf_Capability:

fddRF_Capability:

ue_PowerClass: 4

txRxFrequencySeparation: mhz190_TxRxFrequencySeparation [enum=0]

tddRF_Capability: Omitted

physicalChannelCapability:

fddPhysChCapability:

downlinkPhysChCapability:

maxNoDPCH_PDSCH_Codes: 3

maxNoPhysChBitsReceived: b9600_MaxNoPhysChBitsReceived [enum=6]

supportForSF_512: 0

supportOfPDSCH: 0

simultaneousSCCPCH_DPCH_Reception:

notSupported: NULL

uplinkPhysChCapability:

maxNoDPDCH_BitsTransmitted: b2400_MaxNoDPDCH_BitsTransmitted [enum=2]

supportOfPCPCH: 0

tddPhysChCapability: Omitted

ue_MultiModeRAT_Capability:

multiRAT_CapabilityList:

supportOfGSM: 0

supportOfMulticarrier: 0

multiModeCapability: fdd_MultiModeCapability [enum=1]

securityCapability:

cipheringAlgorithmCap: 0000000000000001

integrityProtectionAlgorithmCap: 0000000000000010

ue_positioning_Capability:

standaloneLocMethodsSupported: 0

ue_BasedOTDOA_Supported: 0

networkAssistedGPS_Supported: noNetworkAssistedGPS_NetworkAssistedGPS_Supported [enum=3]

supportForUE_GPS_TimingOfCellFrames: 0

supportForIPDL: 0

measurementCapability:

downlinkCompressedMode:

fdd_Measurements: 1

tdd_Measurements: Omitted

gsm_Measurements:

gsm900: 1

dcs1800: 1

gsm1900: 0

multiCarrierMeasurements: 0

uplinkCompressedMode:

fdd_Measurements: 1

tdd_Measurements: Omitted

gsm_Measurements:

gsm900: 1

dcs1800: 1

gsm1900: 0

multiCarrierMeasurements: 0

ue_RATSpecificCapability: Omitted

v370NonCriticalExtensions: Omitted

Layer 3 SDU:

[0]4A 0C 00 00 80 00 05 E2
[8]34 1A 20 90 98 CD 08 C5
[16]92 60 41 00 01 00 02 31
[24]F1 F0

#### MAC_DATA_REQ

RLC MAC @ 00:01:04.060

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 15

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 20 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:2

#### PHY_DATA_REQ

MAC PHY @ 00:01:04.060

BTS unit: 1:1
Channel No: 0 Name: FACH
CFN: 15

Message Details:

TFI:1
TB set size:168
TB size:168
TB set (raw):

[0]D0 00 11 02 00 20 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00 00 00

TB set (decoded):

TB 0:

TCTF:3
UEID type:C-RNTI
UEID:1
C/T:1
MAC SDU (144 bits):

[0]02 00 20 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### RLC_AM_DATA_IND

LLA RRC @ 00:01:04.080

Channel ID: Rb2
Cell ID: -1

Message Details:

RLC_AM_DATA_IND:

cellId:-1

routingInfo:

rB_Identity:2

integrityResult:

integrityUsed (IntegrityStatus):i_pass

aM_message:

uL_DCCH_Message:

integrityCheckInfo: Omit

message: (UL_DCCH_MessageType)

rrcConnectionSetupComplete:

rrc_TransactionIdentifier:0

startList:

STARTSingle:

cn_DomainIdentity:ps_domain
start_Value:00000000000000000010

STARTSingle:

cn_DomainIdentity:cs_domain
start_Value:00000000000000000010

ue_RadioAccessCapability:

accessStratumReleaseIndicator:r99

pdcp_Capability:

losslessSRNS_RelocationSupport:true

supportForRfc2507:

supported (MaxHcContextSpace):by8192

rlc_Capability:

totalRLC_AM_BufferSize:kb50
maximumRLC_WindowSize:mws2047
maximumAM_EntityNumber (MaximumAM_EntityNumberRLC_Cap):am6

transportChannelCapability:

dl_TransChCapability:

maxNoBitsReceived (MaxNoBits):b5120
maxConvCodeBitsReceived (MaxNoBits):b1280

turboDecodingSupport: (TurboSupport)

supported (MaxNoBits):b5120

maxSimultaneousTransChs (MaxSimultaneousTransChsDL):e8
maxSimultaneousCCTrCH_Count:1
maxReceivedTransportBlocks (MaxTransportBlocksDL):tb16
maxNumberOfTFC (MaxNumberOfTFC_DL):tfc96
maxNumberOfTF:tf64

ul_TransChCapability:

maxNoBitsTransmitted (MaxNoBits):b3840
maxConvCodeBitsTransmitted (MaxNoBits):b1280

turboEncodingSupport: (TurboSupport)

supported (MaxNoBits):b3840

maxSimultaneousTransChs (MaxSimultaneousTransChsUL):e8

modeSpecificInfo:

fdd:

maxTransmittedBlocks (MaxTransportBlocksUL):tb8
maxNumberOfTFC (MaxNumberOfTFC_UL):tfc32
maxNumberOfTF:tf32

rf_Capability:

fddRF_Capability:

ue_PowerClass:4
txRxFrequencySeparation:mhz190

tddRF_Capability: Omit

physicalChannelCapability:

fddPhysChCapability:

downlinkPhysChCapability: (DL_PhysChCapabilityFDD)

maxNoDPCH_PDSCH_Codes:3
maxNoPhysChBitsReceived:b9600
supportForSF_512:false
supportOfPDSCH:false

simultaneousSCCPCH_DPCH_Reception:

notSupported:

uplinkPhysChCapability: (UL_PhysChCapabilityFDD)

maxNoDPDCH_BitsTransmitted:b2400
supportOfPCPCH:false

tddPhysChCapability: Omit

ue_MultiModeRAT_Capability:

multiRAT_CapabilityList: (MultiRAT_Capability)

supportOfGSM:false
supportOfMulticarrier:false

multiModeCapability:fdd

securityCapability:

cipheringAlgorithmCap:0000000000000001
integrityProtectionAlgorithmCap:0000000000000010

ue_positioning_Capability:

standaloneLocMethodsSupported:false
ue_BasedOTDOA_Supported:false
networkAssistedGPS_Supported:noNetworkAssistedGPS
supportForUE_GPS_TimingOfCellFrames:false
supportForIPDL:false

measurementCapability:

downlinkCompressedMode: (CompressedModeMeasCapability)

fdd_Measurements:true
tdd_Measurements: Omit

gsm_Measurements:

gsm900:true
dcs1800:true
gsm1900:false

multiCarrierMeasurements:false

uplinkCompressedMode: (CompressedModeMeasCapability)

fdd_Measurements:true
tdd_Measurements: Omit

gsm_Measurements:

gsm900:true
dcs1800:true
gsm1900:false

multiCarrierMeasurements:false

ue_RATSpecificCapability: (InterRAT_UE_RadioAccessCapabilityList) Omit

v370NonCriticalExtensions: Omit

#### PHY_DATA_IND

PHY MAC @ 00:01:04.140

BTS unit: 1:1
Channel No: 0 Name: U_RACH
CFN: 3

Message Details:

TFI:0
TB set size:168
TB size:168
TB set (raw):

[0]50 00 12 80 00 15 84 D1
[8]01 00 40 08 17 2A 00 98
[16]38 10 2F A0 91 00

TB set (decoded):

TB 0:

TCTF:1
UEID type:C-RNTI
UEID:1
C/T:2
MAC SDU (144 bits):

[0]80 00 15 84 D1 01 00 40
[8]08 17 2A 00 98 38 10 2F
[16]A0 91

#### MAC_DATA_IND

MAC RLC @ 00:01:04.140

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 3

Message Details:

RLC PDU size (bits):142
RLC PDU (raw):

[0]80 00 15 84 D1 01 00 40
[8]08 17 2A 00 98 38 10 2F
[16]A0 91

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:0
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]15 84 D1 01 00 40 08 17
[8]2A 00 98 38 10 2F A0 91

#### PHY_DATA_IND

PHY MAC @ 00:01:04.200

BTS unit: 1:1
Channel No: 0 Name: U_RACH
CFN: 9

Message Details:

TFI:0
TB set size:168
TB size:168
TB set (raw):

[0]50 00 12 80 08 A2 B3 C0
[8]07 88 80 00 08 28 50 A7
[16]9C 11 9A 60 19 00

TB set (decoded):

TB 0:

TCTF:1
UEID type:C-RNTI
UEID:1
C/T:2
MAC SDU (144 bits):

[0]80 08 A2 B3 C0 07 88 80
[8]00 08 28 50 A7 9C 11 9A
[16]60 19

#### MAC_DATA_IND

MAC RLC @ 00:01:04.200

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 9

Message Details:

RLC PDU size (bits):142
RLC PDU (raw):

[0]80 08 A2 B3 C0 07 88 80
[8]00 08 28 50 A7 9C 11 9A
[16]60 19

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:1
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]A2 B3 C0 07 88 80 00 08
[8]28 50 A7 9C 11 9A 60 19

#### PHY_DATA_IND

PHY MAC @ 00:01:04.260

BTS unit: 1:1
Channel No: 0 Name: U_RACH
CFN: 15

Message Details:

TFI:0
TB set size:168
TB size:168
TB set (raw):

[0]50 00 12 80 15 13 FE 31
[8]E5 03 00 B8 B2 00 00 40
[16]55 55 55 55 55 00

TB set (decoded):

TB 0:

TCTF:1
UEID type:C-RNTI
UEID:1
C/T:2
MAC SDU (144 bits):

[0]80 15 13 FE 31 E5 03 00
[8]B8 B2 00 00 40 55 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:01:04.260

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 15

Message Details:

RLC PDU size (bits):142
RLC PDU (raw):

[0]80 15 13 FE 31 E5 03 00
[8]B8 B2 00 00 40 55 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:2
Polling bit:1 (request a status report)
Length indicator 0 (octets):9
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (9 octets):

[0]31 E5 03 00 B8 B2 00 00
[8]40
Padding associated with length indicator 1 (5 octets):

[0]55 55 55 55 55

#### RLC_AM_DATA_IND: initialDirectTransfer

RLC RRC @ 00:01:04.270

Channel No: 3 Name: DCCH

Message Details:

UL_DCCH_Message:

integrityCheckInfo: Omitted

message:

initialDirectTransfer:

cn_DomainIdentity: ps_domain_CN_DomainIdentity [enum=1]

intraDomainNasNodeSelector:

version:

release99:

cn_Type:

gsm_Map_IDNNS:

routingbasis:

tMSIofsamePLMN:

routingparameter: 0011010001

enteredparameter: 0

nas_Message: 080102E54013070205F41234567800F1100001050A14F382334C03263CA0601716

measuredResultsOnRACH: Omitted

v3a0NonCriticalExtensions:

initialDirectTransfer_v3a0ext:

start_Value: 00000000000000000010

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]15 84 D1 01 00 40 08 17
[8]2A 00 98 38 10 2F A0 91
[16]A2 B3 C0 07 88 80 00 08
[24]28 50 A7 9C 11 9A 60 19
[32]31 E5 03 00 B8 B2 00 00
[40]40

#### RRC_DATA_IND: gmm:attachRequest

RRC NAS @ 00:01:04.270

Cell ID: -1

Message Details:

ATTACHREQUEST:

skipIndicator: 0000

gMMProtocolDiscriminator: 1000

msgType: 00000001

msNetworkCap:

iel: 02

value: E540

gprsCiphKeySeqNo:

spare1: 0

keySeq: 001

attachType:

for: 0

type: 011

drxParameter:

splitPGcycleCode: 00000111

cnDRXcoef: 0000

splitOnCCCH: 0

nonDRXtimer: 010

ptmsiORimsi:

iel: 05

iDigit1: 1111

oddEvenInd: 0

typeOfId: 100

otherDigits: 12345678

oldRAI:

plmn: 00F110

lac: 0001

rac: 05

msRadioAccessCap:

iel: 0A

value: 14F382334C03263CA060

oldPTMSI_Signature: Omitted

readyTimer:

iei: 00010111

unit: 000

value: 10110

tmsiStatus: Omitted

#### MAC_DATA_REQ

RLC MAC @ 00:01:04.270

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 36

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:3

#### PHY_DATA_REQ

MAC PHY @ 00:01:04.270

BTS unit: 1:1
Channel No: 0 Name: FACH
CFN: 36

Message Details:

TFI:1
TB set size:168
TB size:168
TB set (raw):

[0]D0 00 12 02 00 30 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00 00 00

TB set (decoded):

TB 0:

TCTF:3
UEID type:C-RNTI
UEID:1
C/T:2
MAC SDU (144 bits):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### RRC_DATA_REQ: gmm:authenticationAndCipheringRequest

NAS RRC @ 00:01:04.280

Cell ID: -1

Message Details:

AUTHENTICATIONANDCIPHERINGREQUEST:

skipIndicator: 0000

gMMProtocolDiscriminator: 1000

msgType: 00010010

imeisvReq:

spare1: 0

value: 000

ciphAlgorithm:

spare1: 0

algorithm: 001

acRefNo:

value: 0011

forceToStandby:

spare: 0

value: 000

authRand:

iei: 00100001

randValue: 01010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101

gprsCiphKeySeqNo:

iei: 1000

spare1: 0

keySeq: 000

aUTN:

iei: 00101000

iel: 10

aUTN: 01100110000100010000000000110011001000101101110100000000000000000101010101000100011101110110011000010001000000000011001100100010

#### RLC_AM_DATA_REQ:downlinkDirectTransfer

RRC RLC @ 00:01:04.290

Channel No: 3 Name: DCCH

Message Details:

Opt1: 0

Opt2: 0

DL_DCCH_Message:

integrityCheckInfo: Omitted

message:

downlinkDirectTransfer:

r3:

downlinkDirectTransfer_r3:

rrc_TransactionIdentifier: 0

cn_DomainIdentity: ps_domain_CN_DomainIdentity [enum=1]

nas_Message: 0812013021555555555555555555555555555555558028106611003322DD00005544776611003322

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]14 20 4E 10 24 02 60 42
[8]AA AA AA AA AA AA AA AA
[16]AA AA AA AA AA AA AA AB
[24]00 50 20 CC 22 00 66 45
[32]BA 00 00 AA 88 EE CC 22
[40]00 66 44

#### MAC_DATA_REQ

RLC MAC @ 00:01:04.300

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 39

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 00 14 20 4E 10 24 02
[8]60 42 AA AA AA AA AA AA
[16]AA AA

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:0
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]14 20 4E 10 24 02 60 42
[8]AA AA AA AA AA AA AA AA

#### MAC_DATA_REQ

RLC MAC @ 00:01:04.300

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 39

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 08 AA AA AA AA AA AA
[8]AA AB 00 50 20 CC 22 00
[16]66 45

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:1
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]AA AA AA AA AA AA AA AB
[8]00 50 20 CC 22 00 66 45

#### MAC_DATA_REQ

RLC MAC @ 00:01:04.300

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 39

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 15 17 FE BA 00 00 AA
[8]88 EE CC 22 00 66 44 00
[16]00 00

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:2
Polling bit:1 (request a status report)
Length indicator 0 (octets):11
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (11 octets):

[0]BA 00 00 AA 88 EE CC 22
[8]00 66 44
Padding associated with length indicator 1 (3 octets):

[0]00 00 00

#### PHY_DATA_REQ

MAC PHY @ 00:01:04.300

BTS unit: 1:1
Channel No: 0 Name: FACH
CFN: 39

Message Details:

TFI:2
TB set size:336
TB size:168
TB set (raw, each TB word aligned):

[0]D0 00 12 80 00 14 20 4E
[8]10 24 02 60 42 AA AA AA
[16]AA AA AA AA AA 00 D0 00
[24]12 80 08 AA AA AA AA AA
[32]AA AA AB 00 50 20 CC 22
[40]00 66 45 00

TB set (decoded):

TB 0:

TCTF:3
UEID type:C-RNTI
UEID:1
C/T:2
MAC SDU (144 bits):

[0]80 00 14 20 4E 10 24 02
[8]60 42 AA AA AA AA AA AA
[16]AA AA

TB 1:

TCTF:3
UEID type:C-RNTI
UEID:1
C/T:2
MAC SDU (144 bits):

[0]80 08 AA AA AA AA AA AA
[8]AA AB 00 50 20 CC 22 00
[16]66 45

#### PHY_DATA_REQ

MAC PHY @ 00:01:04.310

BTS unit: 1:1
Channel No: 0 Name: FACH
CFN: 40

Message Details:

TFI:1
TB set size:168
TB size:168
TB set (raw):

[0]D0 00 12 80 15 17 FE BA
[8]00 00 AA 88 EE CC 22 00
[16]66 44 00 00 00 00

TB set (decoded):

TB 0:

TCTF:3
UEID type:C-RNTI
UEID:1
C/T:2
MAC SDU (144 bits):

[0]80 15 17 FE BA 00 00 AA
[8]88 EE CC 22 00 66 44 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:01:04.540

BTS unit: 1:1
Channel No: 0 Name: U_RACH
CFN: 43

Message Details:

TFI:0
TB set size:168
TB size:168
TB set (raw):

[0]50 00 12 02 00 30 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00 00 00

TB set (decoded):

TB 0:

TCTF:1
UEID type:C-RNTI
UEID:1
C/T:2
MAC SDU (144 bits):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### MAC_DATA_IND

MAC RLC @ 00:01:04.540

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 43

Message Details:

RLC PDU size (bits):142
RLC PDU (raw):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:3

#### PHY_DATA_IND

PHY MAC @ 00:01:04.680

BTS unit: 1:1
Channel No: 0 Name: U_RACH
CFN: 57

Message Details:

TFI:0
TB set size:168
TB size:168
TB set (raw):

[0]50 00 12 80 18 6C 80 A8
[8]40 98 19 12 AA 23 BB 31
[16]48 60 88 01 99 00

TB set (decoded):

TB 0:

TCTF:1
UEID type:C-RNTI
UEID:1
C/T:2
MAC SDU (144 bits):

[0]80 18 6C 80 A8 40 98 19
[8]12 AA 23 BB 31 48 60 88
[16]01 99

#### MAC_DATA_IND

MAC RLC @ 00:01:04.680

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 57

Message Details:

RLC PDU size (bits):142
RLC PDU (raw):

[0]80 18 6C 80 A8 40 98 19
[8]12 AA 23 BB 31 48 60 88
[16]01 99

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:3
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]6C 80 A8 40 98 19 12 AA
[8]23 BB 31 48 60 88 01 99

#### PHY_DATA_IND

PHY MAC @ 00:01:04.740

BTS unit: 1:1
Channel No: 0 Name: U_RACH
CFN: 63

Message Details:

TFI:0
TB set size:168
TB size:168
TB set (raw):

[0]50 00 12 80 25 13 FE 16
[8]EE 67 FF 74 CC 45 DD 50
[16]55 55 55 55 55 00

TB set (decoded):

TB 0:

TCTF:1
UEID type:C-RNTI
UEID:1
C/T:2
MAC SDU (144 bits):

[0]80 25 13 FE 16 EE 67 FF
[8]74 CC 45 DD 50 55 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:01:04.740

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 63

Message Details:

RLC PDU size (bits):142
RLC PDU (raw):

[0]80 25 13 FE 16 EE 67 FF
[8]74 CC 45 DD 50 55 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:4
Polling bit:1 (request a status report)
Length indicator 0 (octets):9
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (9 octets):

[0]16 EE 67 FF 74 CC 45 DD
[8]50
Padding associated with length indicator 1 (5 octets):

[0]55 55 55 55 55

#### RLC_AM_DATA_IND: uplinkDirectTransfer

RLC RRC @ 00:01:04.750

Channel No: 3 Name: DCCH

Message Details:

UL_DCCH_Message:

integrityCheckInfo: Omitted

message:

uplinkDirectTransfer:

cn_DomainIdentity: ps_domain_CN_DomainIdentity [enum=1]

nas_Message: 0813032255447766290C11003322DDCCFFEE9988BBAA

measuredResultsOnRACH: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]6C 80 A8 40 98 19 12 AA
[8]23 BB 31 48 60 88 01 99
[16]16 EE 67 FF 74 CC 45 DD
[24]50

#### RRC_DATA_IND: gmm:authenticationAndCipheringResponse

RRC NAS @ 00:01:04.750

Cell ID: -1

Message Details:

AUTHENTICATIONANDCIPHERINGRESPONSE:

skipIndicator: 0000

gMMProtocolDiscriminator: 1000

msgType: 00010011

spare4: 0000

acRefNo:

value: 0011

authRsp:

iei: 00100010

value: 01010101010001000111011101100110

imeisv: Omitted

authRspExt:

iei: 00101001

iel: 0C

rES: 000100010000000000110011001000101101110111001100111111111110111010011001100010001011101110101010

#### CRLC_SecurityMode_Config_REQ

RRC LLA @ 00:01:04.750

Cell ID: -1

Message Details:

CRLC_SecurityMode_Config_REQ:

cellId:-1

rlcSecurityInfo: (SecurityInfo)

cn_DomainIdentity:ps_domain
startValue (START_Value):00000000000000000000
cipheringKey:01000100011101110110011000010001000000000011001100100010110111011100110011111111111011101001100110001000101110111010101001010101
integrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
gsmCipheringKey: Omit

#### CRLC_SecurityMode_Config_REQ

RRC RLC @ 00:01:04.750

Message Details:

cellIdentity: 1

rlcSecurityInfo:

cn_DomainIdentity: ps_domain_CN_DomainIdentity

startValue: 00000000000000000000

cipheringKey: 01000100011101110110011000010001000000000011001100100010110111011100110011111111111011101001100110001000101110111010101001010101

integrityKey: 01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100

#### MAC_DATA_REQ

RLC MAC @ 00:01:04.750

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 84

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 50 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:5

#### PHY_DATA_REQ

MAC PHY @ 00:01:04.750

BTS unit: 1:1
Channel No: 0 Name: FACH
CFN: 84

Message Details:

TFI:1
TB set size:168
TB size:168
TB set (raw):

[0]D0 00 12 02 00 50 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00 00 00

TB set (decoded):

TB 0:

TCTF:3
UEID type:C-RNTI
UEID:1
C/T:2
MAC SDU (144 bits):

[0]02 00 50 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### CRLC_SecurityMode_Config_CNF

LLA RRC @ 00:01:04.760

Cell ID: -1

Message Details:

CRLC_SecurityMode_Config_CNF:

cellId:-1

#### CRLC_SetRRC_MessageSN_REQ

RRC LLA @ 00:01:04.760

Channel ID: Rb0
Cell ID: 0

Message Details:

CRLC_SetRRC_MessageSN_REQ:

cellId:0

routingInfo:

rB_Identity:0

count_I_LSB_UL (RRC_SequenceNumber): Omit
count_I_LSB_DL (RRC_SequenceNumber):0

#### CRLC_SetRRC_MessageSN_CNF

LLA RRC @ 00:01:04.780

Channel ID: Rb0
Cell ID: 0

Message Details:

CRLC_SetRRC_MessageSN_CNF:

cellId:0

routingInfo:

rB_Identity:0

#### CRLC_SetRRC_MessageSN_REQ

RRC LLA @ 00:01:04.780

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_REQ:

cellId:-1

routingInfo:

rB_Identity:1

count_I_LSB_UL (RRC_SequenceNumber): Omit
count_I_LSB_DL (RRC_SequenceNumber):0

#### CRLC_SetRRC_MessageSN_CNF

LLA RRC @ 00:01:04.790

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_CNF:

cellId:-1

routingInfo:

rB_Identity:1

#### CRLC_SetRRC_MessageSN_REQ

RRC LLA @ 00:01:04.790

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_REQ:

cellId:-1

routingInfo:

rB_Identity:2

count_I_LSB_UL (RRC_SequenceNumber): Omit
count_I_LSB_DL (RRC_SequenceNumber):0

#### CRLC_SetRRC_MessageSN_CNF

LLA RRC @ 00:01:04.810

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_CNF:

cellId:-1

routingInfo:

rB_Identity:2

#### CRLC_SetRRC_MessageSN_REQ

RRC LLA @ 00:01:04.810

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_REQ:

cellId:-1

routingInfo:

rB_Identity:3

count_I_LSB_UL (RRC_SequenceNumber): Omit
count_I_LSB_DL (RRC_SequenceNumber):0

#### CRLC_SetRRC_MessageSN_CNF

LLA RRC @ 00:01:04.830

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_CNF:

cellId:-1

routingInfo:

rB_Identity:3

#### CRLC_SetRRC_MessageSN_REQ

RRC LLA @ 00:01:04.830

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_REQ:

cellId:-1

routingInfo:

rB_Identity:4

count_I_LSB_UL (RRC_SequenceNumber): Omit
count_I_LSB_DL (RRC_SequenceNumber):0

#### CRLC_SetRRC_MessageSN_CNF

LLA RRC @ 00:01:04.840

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_CNF:

cellId:-1

routingInfo:

rB_Identity:4

#### CRLC_Integrity_Activate_REQ

RRC LLA @ 00:01:04.840

Cell ID: -1

Message Details:

CRLC_Integrity_Activate_REQ:

cellId:-1
cn_DomainIdentity:ps_domain

integrityActivationInfo:

integrityProtectionModeInfo:

integrityProtectionModeCommand:

startIntegrityProtection:

integrityProtInitNumber:00001111000011110000111100001111

integrityProtectionAlgorithm:uia1

#### CRLC_Integrity_Activate_REQ

RRC RLC @ 00:01:04.840

Message Details:

cellIdentity: 1

integrityActivationInfo:

integrityProtectionModeInfo:

integrityProtectionModeCommand:

startIntegrityProtection:

integrityProtInitNumber: 00001111000011110000111100001111

#### CRLC_Integrity_Activate_CNF

LLA RRC @ 00:01:04.860

Cell ID: -1

Message Details:

CRLC_Integrity_Activate_CNF:

cellId:-1

#### CRLC_SequenceNumber_REQ

RRC LLA @ 00:01:04.860

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_SequenceNumber_REQ:

cellId:-1

routingInfo:

rB_Identity:1

#### CRLC Sequence Number CNF

RLC RRC @ 00:01:04.880

BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 97

Message Details:

Sequence Number Results:

DL Count C:00000000000000000000000000000000
UL Count C:00000000000000000000000000000000

#### CRLC_SequenceNumber_CNF

LLA RRC @ 00:01:04.890

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_SequenceNumber_CNF:

cellId:-1

routingInfo:

rB_Identity:1

count_C_MSB_UL (COUNT_C_MSB):0
count_C_LSB_UL (RLC_SequenceNumber):0
count_C_MSB_DL (COUNT_C_MSB):0
count_C_LSB_DL (RLC_SequenceNumber):0

#### CRLC_SequenceNumber_REQ

RRC LLA @ 00:01:04.890

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_SequenceNumber_REQ:

cellId:-1

routingInfo:

rB_Identity:2

#### CRLC Sequence Number CNF

RLC RRC @ 00:01:04.910

BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 100

Message Details:

Sequence Number Results:

DL Count C:00000000000000000000000000000000
UL Count C:00000000000000000000000000000010

#### CRLC_SequenceNumber_CNF

LLA RRC @ 00:01:04.920

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_SequenceNumber_CNF:

cellId:-1

routingInfo:

rB_Identity:2

count_C_MSB_UL (COUNT_C_MSB):0
count_C_LSB_UL (RLC_SequenceNumber):2
count_C_MSB_DL (COUNT_C_MSB):0
count_C_LSB_DL (RLC_SequenceNumber):0

#### CRLC_SequenceNumber_REQ

RRC LLA @ 00:01:04.920

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_SequenceNumber_REQ:

cellId:-1

routingInfo:

rB_Identity:3

#### CRLC Sequence Number CNF

RLC RRC @ 00:01:04.940

BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 103

Message Details:

Sequence Number Results:

DL Count C:00000000000000000000000000000011
UL Count C:00000000000000000000000000000101

#### CRLC_SequenceNumber_CNF

LLA RRC @ 00:01:04.940

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_SequenceNumber_CNF:

cellId:-1

routingInfo:

rB_Identity:3

count_C_MSB_UL (COUNT_C_MSB):0
count_C_LSB_UL (RLC_SequenceNumber):5
count_C_MSB_DL (COUNT_C_MSB):0
count_C_LSB_DL (RLC_SequenceNumber):3

#### CRLC_SequenceNumber_REQ

RRC LLA @ 00:01:04.940

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_SequenceNumber_REQ:

cellId:-1

routingInfo:

rB_Identity:4

#### CRLC Sequence Number CNF

RLC RRC @ 00:01:04.950

BTS unit: 1:1
Channel No: 4 Name: DCCH
CFN: 104

Message Details:

Sequence Number Results:

DL Count C:00000000000000000000000000000000
UL Count C:00000000000000000000000000000000

#### CRLC_SequenceNumber_CNF

LLA RRC @ 00:01:04.950

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_SequenceNumber_CNF:

cellId:-1

routingInfo:

rB_Identity:4

count_C_MSB_UL (COUNT_C_MSB):0
count_C_LSB_UL (RLC_SequenceNumber):0
count_C_MSB_DL (COUNT_C_MSB):0
count_C_LSB_DL (RLC_SequenceNumber):0

#### CRLC_Suspend_REQ

RRC LLA @ 00:01:04.950

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Suspend_REQ:

cellId:-1

routingInfo:

rB_Identity:1

n (RLC_SequenceNumber):0

#### CRLC Suspend REQ

LLA RLC @ 00:01:04.960

BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 105

Message Details:

N:0

#### CRLC Suspend CNF

RLC LLA @ 00:01:04.960

BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 105

Message Details:

Sequence Number:0

#### CRLC_Suspend_CNF

LLA RRC @ 00:01:04.970

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Suspend_CNF:

cellId:-1

routingInfo:

rB_Identity:1

vt (RLC_SequenceNumber):0

#### CRLC_Suspend_REQ

RRC LLA @ 00:01:04.970

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Suspend_REQ:

cellId:-1

routingInfo:

rB_Identity:3

n (RLC_SequenceNumber):3

#### CRLC Suspend REQ

LLA RLC @ 00:01:04.970

BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 106

Message Details:

N:3

#### CRLC Suspend CNF

RLC LLA @ 00:01:04.970

BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 106

Message Details:

Sequence Number:3

#### CRLC_Suspend_CNF

LLA RRC @ 00:01:04.980

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Suspend_CNF:

cellId:-1

routingInfo:

rB_Identity:3

vt (RLC_SequenceNumber):3

#### CRLC_Suspend_REQ

RRC LLA @ 00:01:04.980

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Suspend_REQ:

cellId:-1

routingInfo:

rB_Identity:4

n (RLC_SequenceNumber):0

#### CRLC Suspend REQ

LLA RLC @ 00:01:04.990

BTS unit: 1:1
Channel No: 4 Name: DCCH
CFN: 108

Message Details:

N:0

#### CRLC Suspend CNF

RLC LLA @ 00:01:04.990

BTS unit: 1:1
Channel No: 4 Name: DCCH
CFN: 108

Message Details:

Sequence Number:0

#### CRLC_Suspend_CNF

LLA RRC @ 00:01:05.000

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Suspend_CNF:

cellId:-1

routingInfo:

rB_Identity:4

vt (RLC_SequenceNumber):0

#### CRLC_Ciphering_Activate_REQ

RRC LLA @ 00:01:05.000

Cell ID: -1

Message Details:

CRLC_Ciphering_Activate_REQ:

cellId:-1
ratType:fdd
cn_DomainIdentity:ps_domain

ciphActivationInfo:

cipheringModeInfo:

cipheringModeCommand:

startRestart (CipheringAlgorithm):uea0

activationTimeForDPCH (ActivationTime): Omit

rb_DL_CiphActivationTimeInfo: (RB_ActivationTimeInfoList)

RB_ActivationTimeInfo:

rb_Identity:1
rlc_SequenceNumber:0

incHFN (RLC_IncMode):notInc

#### CRLC_Ciphering_Activate_CNF

LLA RRC @ 00:01:05.010

Cell ID: -1

Message Details:

CRLC_Ciphering_Activate_CNF:

cellId:-1

#### CRLC_Ciphering_Activate_REQ

RRC LLA @ 00:01:05.010

Cell ID: -1

Message Details:

CRLC_Ciphering_Activate_REQ:

cellId:-1
ratType:fdd
cn_DomainIdentity:ps_domain

ciphActivationInfo:

cipheringModeInfo:

cipheringModeCommand:

startRestart (CipheringAlgorithm):uea0

activationTimeForDPCH (ActivationTime): Omit

rb_DL_CiphActivationTimeInfo: (RB_ActivationTimeInfoList)

RB_ActivationTimeInfo:

rb_Identity:2
rlc_SequenceNumber:2

incHFN (RLC_IncMode):notInc

#### CRLC_Ciphering_Activate_CNF

LLA RRC @ 00:01:05.030

Cell ID: -1

Message Details:

CRLC_Ciphering_Activate_CNF:

cellId:-1

#### CRLC_Ciphering_Activate_REQ

RRC LLA @ 00:01:05.030

Cell ID: -1

Message Details:

CRLC_Ciphering_Activate_REQ:

cellId:-1
ratType:fdd
cn_DomainIdentity:ps_domain

ciphActivationInfo:

cipheringModeInfo:

cipheringModeCommand:

startRestart (CipheringAlgorithm):uea0

activationTimeForDPCH (ActivationTime): Omit

rb_DL_CiphActivationTimeInfo: (RB_ActivationTimeInfoList)

RB_ActivationTimeInfo:

rb_Identity:3
rlc_SequenceNumber:3

incHFN (RLC_IncMode):notInc

#### CRLC_Ciphering_Activate_CNF

LLA RRC @ 00:01:05.040

Cell ID: -1

Message Details:

CRLC_Ciphering_Activate_CNF:

cellId:-1

#### CRLC_Ciphering_Activate_REQ

RRC LLA @ 00:01:05.040

Cell ID: -1

Message Details:

CRLC_Ciphering_Activate_REQ:

cellId:-1
ratType:fdd
cn_DomainIdentity:ps_domain

ciphActivationInfo:

cipheringModeInfo:

cipheringModeCommand:

startRestart (CipheringAlgorithm):uea0

activationTimeForDPCH (ActivationTime): Omit

rb_DL_CiphActivationTimeInfo: (RB_ActivationTimeInfoList)

RB_ActivationTimeInfo:

rb_Identity:4
rlc_SequenceNumber:0

incHFN (RLC_IncMode):notInc

#### CRLC_Ciphering_Activate_CNF

LLA RRC @ 00:01:05.060

Cell ID: -1

Message Details:

CRLC_Ciphering_Activate_CNF:

cellId:-1

#### CRLC_Integrity_Activate_REQ

RRC LLA @ 00:01:05.060

Cell ID: -1

Message Details:

CRLC_Integrity_Activate_REQ:

cellId:-1
cn_DomainIdentity:ps_domain

integrityActivationInfo:

ul_IntegProtActivationInfo: (IntegrityProtActivationInfoList)

SS_IntegrityProtActivationTimeInfo:

rb_Identity:2
rrc_MessageSequenceNumber:0

#### CMAC Integrity Check Request

RRC MAC @ 00:01:05.080

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000001
Data:

[0]00 00 00 01
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:1 (RNC to UE)
Message Length (bits):200
Message:

[0]80 00 00 01 04 0C 00 00
[8]80 01 20 C0 00 01 00 21
[16]00 18 C0 02 0F 0F 0F 0F
[24]80

#### CMAC Integrity Check Result

MAC RRC @ 00:01:05.080

Message Details:

Integrity Check Result:

MAC-I:01110001101111100101001001010100
Data:

[0]71 BE 52 54

#### CRLC_Integrity_Activate_CNF

LLA RRC @ 00:01:05.080

Cell ID: -1

Message Details:

CRLC_Integrity_Activate_CNF:

cellId:-1

#### RLC_AM_DATA_REQ

RRC LLA @ 00:01:05.080

Channel ID: Rb2
Cell ID: -1

Message Details:

RLC_AM_DATA_REQ:

cellId:-1

routingInfo:

rB_Identity:2

confirmationRequest: (AmConfirmationRequest)

noConfirmationRequest:

aM_message:

dL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode:00000000000000000000000000000000
rrc_MessageSequenceNumber:0

message: (DL_DCCH_MessageType)

securityModeCommand:

r3:

securityModeCommand_r3: (SecurityModeCommand_r3_IEs)

rrc_TransactionIdentifier:0

securityCapability:

cipheringAlgorithmCap:0000000000000001
integrityProtectionAlgorithmCap:0000000000000010

cipheringModeInfo:

cipheringModeCommand:

startRestart (CipheringAlgorithm):uea0

activationTimeForDPCH (ActivationTime): Omit

rb_DL_CiphActivationTimeInfo: (RB_ActivationTimeInfoList)

RB_ActivationTimeInfo:

rb_Identity:1
rlc_SequenceNumber:0

RB_ActivationTimeInfo:

rb_Identity:2
rlc_SequenceNumber:2

RB_ActivationTimeInfo:

rb_Identity:3
rlc_SequenceNumber:3

RB_ActivationTimeInfo:

rb_Identity:4
rlc_SequenceNumber:0

integrityProtectionModeInfo:

integrityProtectionModeCommand:

startIntegrityProtection:

integrityProtInitNumber:00001111000011110000111100001111

integrityProtectionAlgorithm:uia1

cn_DomainIdentity:ps_domain

ue_SystemSpecificSecurityCap: (InterRAT_UE_SecurityCapList) Omit

laterNonCriticalExtensions: Omit

#### RLC_AM_DATA_REQ: securityModeCommand

LLA RLC @ 00:01:05.080

Channel No: 2 Name: DCCH

Message Details:

DL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode: 01110001101111100101001001010100

rrc_MessageSequenceNumber: 1

message:

securityModeCommand:

r3:

securityModeCommand_r3:

rrc_TransactionIdentifier: 0

securityCapability:

cipheringAlgorithmCap: 0000000000000001

integrityProtectionAlgorithmCap: 0000000000000010

cipheringModeInfo:

cipheringModeCommand:

startRestart: uea0_CipheringAlgorithm [enum=0]

activationTimeForDPCH: Omitted

rb_DL_CiphActivationTimeInfo:

RB_ActivationTimeInfoList.element:

rb_Identity: 1

rlc_SequenceNumber: 0

RB_ActivationTimeInfoList.element:

rb_Identity: 2

rlc_SequenceNumber: 2

RB_ActivationTimeInfoList.element:

rb_Identity: 3

rlc_SequenceNumber: 3

RB_ActivationTimeInfoList.element:

rb_Identity: 4

rlc_SequenceNumber: 0

integrityProtectionModeInfo:

integrityProtectionModeCommand:

startIntegrityProtection:

integrityProtInitNumber: 00001111000011110000111100001111

integrityProtectionAlgorithm: uia1_IntegrityProtectionAlgorithm [enum=0]

cn_DomainIdentity: ps_domain_CN_DomainIdentity [enum=1]

ue_SystemSpecificSecurityCap: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]B8 DF 29 2A 0C 0C 00 00
[8]80 01 20 C0 00 01 00 21
[16]00 18 C0 02 0F 0F 0F 0F
[24]80

#### MAC_DATA_REQ

RLC MAC @ 00:01:05.090

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 118

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 00 B8 DF 29 2A 0C 0C
[8]00 00 80 01 20 C0 00 01
[16]00 21

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:0
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]B8 DF 29 2A 0C 0C 00 00
[8]80 01 20 C0 00 01 00 21

#### MAC_DATA_REQ

RLC MAC @ 00:01:05.090

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 118

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 0D 13 FE 00 18 C0 02
[8]0F 0F 0F 0F 80 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:1
Polling bit:1 (request a status report)
Length indicator 0 (octets):9
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (9 octets):

[0]00 18 C0 02 0F 0F 0F 0F
[8]80
Padding associated with length indicator 1 (5 octets):

[0]00 00 00 00 00

#### PHY_DATA_REQ

MAC PHY @ 00:01:05.100

BTS unit: 1:1
Channel No: 0 Name: FACH
CFN: 119

Message Details:

TFI:2
TB set size:336
TB size:168
TB set (raw, each TB word aligned):

[0]D0 00 11 80 00 B8 DF 29
[8]2A 0C 0C 00 00 80 01 20
[16]C0 00 01 00 21 00 D0 00
[24]11 80 0D 13 FE 00 18 C0
[32]02 0F 0F 0F 0F 80 00 00
[40]00 00 00 00

TB set (decoded):

TB 0:

TCTF:3
UEID type:C-RNTI
UEID:1
C/T:1
MAC SDU (144 bits):

[0]80 00 B8 DF 29 2A 0C 0C
[8]00 00 80 01 20 C0 00 01
[16]00 21

TB 1:

TCTF:3
UEID type:C-RNTI
UEID:1
C/T:1
MAC SDU (144 bits):

[0]80 0D 13 FE 00 18 C0 02
[8]0F 0F 0F 0F 80 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:01:05.320

BTS unit: 1:1
Channel No: 0 Name: U_RACH
CFN: 121

Message Details:

TFI:0
TB set size:168
TB size:168
TB set (raw):

[0]50 00 11 02 00 20 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00 00 00

TB set (decoded):

TB 0:

TCTF:1
UEID type:C-RNTI
UEID:1
C/T:1
MAC SDU (144 bits):

[0]02 00 20 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### MAC_DATA_IND

MAC RLC @ 00:01:05.320

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 121

Message Details:

RLC PDU size (bits):142
RLC PDU (raw):

[0]02 00 20 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:2

#### PHY_DATA_IND

PHY MAC @ 00:01:05.380

BTS unit: 1:1
Channel No: 0 Name: U_RACH
CFN: 127

Message Details:

TFI:0
TB set size:168
TB size:168
TB set (raw):

[0]50 00 11 80 10 E0 80 BC
[8]C2 0D 31 00 00 01 80 00
[16]02 00 E2 00 51 00

TB set (decoded):

TB 0:

TCTF:1
UEID type:C-RNTI
UEID:1
C/T:1
MAC SDU (144 bits):

[0]80 10 E0 80 BC C2 0D 31
[8]00 00 01 80 00 02 00 E2
[16]00 51

#### MAC_DATA_IND

MAC RLC @ 00:01:05.380

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 127

Message Details:

RLC PDU size (bits):142
RLC PDU (raw):

[0]80 10 E0 80 BC C2 0D 31
[8]00 00 01 80 00 02 00 E2
[16]00 51

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:2
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]E0 80 BC C2 0D 31 00 00
[8]01 80 00 02 00 E2 00 51

#### PHY_DATA_IND

PHY MAC @ 00:01:05.440

BTS unit: 1:1
Channel No: 0 Name: U_RACH
CFN: 133

Message Details:

TFI:0
TB set size:168
TB size:168
TB set (raw):

[0]50 00 11 80 1D 05 FE 80
[8]00 55 55 55 55 55 55 55
[16]55 55 55 55 55 00

TB set (decoded):

TB 0:

TCTF:1
UEID type:C-RNTI
UEID:1
C/T:1
MAC SDU (144 bits):

[0]80 1D 05 FE 80 00 55 55
[8]55 55 55 55 55 55 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:01:05.440

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 133

Message Details:

RLC PDU size (bits):142
RLC PDU (raw):

[0]80 1D 05 FE 80 00 55 55
[8]55 55 55 55 55 55 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:3
Polling bit:1 (request a status report)
Length indicator 0 (octets):2
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (2 octets):

[0]80 00
Padding associated with length indicator 1 (12 octets):

[0]55 55 55 55 55 55 55 55
[8]55 55 55 55

#### MAC_DATA_REQ

RLC MAC @ 00:01:05.450

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 154

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 40 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:4

#### PHY_DATA_REQ

MAC PHY @ 00:01:05.450

BTS unit: 1:1
Channel No: 0 Name: FACH
CFN: 154

Message Details:

TFI:1
TB set size:168
TB size:168
TB set (raw):

[0]D0 00 11 02 00 40 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00 00 00

TB set (decoded):

TB 0:

TCTF:3
UEID type:C-RNTI
UEID:1
C/T:1
MAC SDU (144 bits):

[0]02 00 40 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### CMAC Integrity Check Request

RRC MAC @ 00:01:05.470

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000001
Data:

[0]00 00 00 01
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:0 (UE to RNC)
Message Length (bits):144
Message:

[0]80 00 00 01 05 31 00 00
[8]01 80 00 02 00 E2 00 51
[16]80 00

#### RLC_AM_DATA_IND: securityModeComplete

RLC LLA @ 00:01:05.470

Channel No: 2 Name: DCCH

Message Details:

UL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode: 11000001000000010111100110000100

rrc_MessageSequenceNumber: 1

message:

securityModeComplete:

rrc_TransactionIdentifier: 0

ul_IntegProtActivationInfo:

rrc_MessageSequenceNumberList:

RRC_MessageSequenceNumberList.element: 0

RRC_MessageSequenceNumberList.element: 0

RRC_MessageSequenceNumberList.element: 0

RRC_MessageSequenceNumberList.element: 0

RRC_MessageSequenceNumberList.element: 0

rb_UL_CiphActivationTimeInfo:

RB_ActivationTimeInfoList.element:

rb_Identity: 1

rlc_SequenceNumber: 0

RB_ActivationTimeInfoList.element:

rb_Identity: 2

rlc_SequenceNumber: 7

RB_ActivationTimeInfoList.element:

rb_Identity: 3

rlc_SequenceNumber: 5

RB_ActivationTimeInfoList.element:

rb_Identity: 4

rlc_SequenceNumber: 0

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]E0 80 BC C2 0D 31 00 00
[8]01 80 00 02 00 E2 00 51
[16]80 00

#### CMAC Integrity Check Result

MAC RRC @ 00:01:05.470

Message Details:

Integrity Check Result:

MAC-I:11000001000000010111100110000100
Data:

[0]C1 01 79 84

#### RLC_AM_DATA_IND

LLA RRC @ 00:01:05.470

Channel ID: Rb2
Cell ID: -1

Message Details:

RLC_AM_DATA_IND:

cellId:-1

routingInfo:

rB_Identity:2

integrityResult:

integrityUsed (IntegrityStatus):i_pass

aM_message:

uL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode:11000001000000010111100110000100
rrc_MessageSequenceNumber:1

message: (UL_DCCH_MessageType)

securityModeComplete:

rrc_TransactionIdentifier:0

ul_IntegProtActivationInfo: (IntegrityProtActivationInfo)

rrc_MessageSequenceNumberList:

RRC_MessageSequenceNumber:0
RRC_MessageSequenceNumber:0
RRC_MessageSequenceNumber:0
RRC_MessageSequenceNumber:0
RRC_MessageSequenceNumber:0

rb_UL_CiphActivationTimeInfo: (RB_ActivationTimeInfoList)

RB_ActivationTimeInfo:

rb_Identity:1
rlc_SequenceNumber:0

RB_ActivationTimeInfo:

rb_Identity:2
rlc_SequenceNumber:7

RB_ActivationTimeInfo:

rb_Identity:3
rlc_SequenceNumber:5

RB_ActivationTimeInfo:

rb_Identity:4
rlc_SequenceNumber:0

laterNonCriticalExtensions: Omit

#### CRLC_Ciphering_Activate_REQ

RRC LLA @ 00:01:05.470

Cell ID: -1

Message Details:

CRLC_Ciphering_Activate_REQ:

cellId:-1
ratType:fdd
cn_DomainIdentity:ps_domain

ciphActivationInfo:

rb_UL_CipheringActivationTimeInfo: (RB_ActivationTimeInfoList)

RB_ActivationTimeInfo:

rb_Identity:1
rlc_SequenceNumber:0

RB_ActivationTimeInfo:

rb_Identity:2
rlc_SequenceNumber:7

RB_ActivationTimeInfo:

rb_Identity:3
rlc_SequenceNumber:5

RB_ActivationTimeInfo:

rb_Identity:4
rlc_SequenceNumber:0

incHFN (RLC_IncMode):notInc

#### CRLC UM Ciphering Activate REQ

LLA RLC @ 00:01:05.480

BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 157

Message Details:

Ciphering Parameters:

Mode command:Stop
Type:UM
Radio Bearer identity:0
Downlink activation time:0
Uplink activation time:0

#### CRLC UM Ciphering Activate CNF

RLC LLA @ 00:01:05.480

BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 157

Message Details:

#### CRLC AM Ciphering Activate REQ

LLA RLC @ 00:01:05.490

BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 158

Message Details:

Ciphering Parameters:

Mode command:Stop
Type:AM
Radio Bearer identity:1
Downlink activation time:2
Uplink activation time:7

#### CRLC AM Ciphering Activate CNF

RLC LLA @ 00:01:05.490

BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 158

Message Details:

#### CRLC AM Ciphering Activate REQ

LLA RLC @ 00:01:05.500

BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 159

Message Details:

Ciphering Parameters:

Mode command:Stop
Type:AM
Radio Bearer identity:2
Downlink activation time:3
Uplink activation time:5

#### CRLC AM Ciphering Activate CNF

RLC LLA @ 00:01:05.500

BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 159

Message Details:

#### CRLC AM Ciphering Activate REQ

LLA RLC @ 00:01:05.520

BTS unit: 1:1
Channel No: 4 Name: DCCH
CFN: 161

Message Details:

Ciphering Parameters:

Mode command:Stop
Type:AM
Radio Bearer identity:3
Downlink activation time:0
Uplink activation time:0

#### CRLC AM Ciphering Activate CNF

RLC LLA @ 00:01:05.520

BTS unit: 1:1
Channel No: 4 Name: DCCH
CFN: 161

Message Details:

#### CRLC_Ciphering_Activate_CNF

LLA RRC @ 00:01:05.530

Cell ID: -1

Message Details:

CRLC_Ciphering_Activate_CNF:

cellId:-1

#### CRLC_Integrity_Activate_REQ

RRC LLA @ 00:01:05.530

Cell ID: -1

Message Details:

CRLC_Integrity_Activate_REQ:

cellId:-1
cn_DomainIdentity:ps_domain

integrityActivationInfo:

ul_IntegProtActivationInfo: (IntegrityProtActivationInfoList)

SS_IntegrityProtActivationTimeInfo:

rb_Identity:0
rrc_MessageSequenceNumber:0

SS_IntegrityProtActivationTimeInfo:

rb_Identity:1
rrc_MessageSequenceNumber:0

SS_IntegrityProtActivationTimeInfo:

rb_Identity:3
rrc_MessageSequenceNumber:0

SS_IntegrityProtActivationTimeInfo:

rb_Identity:4
rrc_MessageSequenceNumber:0

#### CRLC_Integrity_Activate_CNF

LLA RRC @ 00:01:05.540

Cell ID: -1

Message Details:

CRLC_Integrity_Activate_CNF:

cellId:-1

#### CRLC_Resume_REQ

RRC LLA @ 00:01:05.540

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Resume_REQ:

cellId:-1

routingInfo:

rB_Identity:1

#### CRLC Resume REQ

LLA RLC @ 00:01:05.550

BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 164

Message Details:

#### CRLC Resume CNF

RLC LLA @ 00:01:05.550

BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 164

Message Details:

#### CRLC_Resume_CNF

LLA RRC @ 00:01:05.560

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Resume_CNF:

cellId:-1

routingInfo:

rB_Identity:1

#### CRLC_Resume_REQ

RRC LLA @ 00:01:05.560

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Resume_REQ:

cellId:-1

routingInfo:

rB_Identity:3

#### CRLC Resume REQ

LLA RLC @ 00:01:05.570

BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 166

Message Details:

#### CRLC Resume CNF

RLC LLA @ 00:01:05.570

BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 166

Message Details:

#### CRLC_Resume_CNF

LLA RRC @ 00:01:05.580

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Resume_CNF:

cellId:-1

routingInfo:

rB_Identity:3

#### CRLC_Resume_REQ

RRC LLA @ 00:01:05.580

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Resume_REQ:

cellId:-1

routingInfo:

rB_Identity:4

#### CRLC Resume REQ

LLA RLC @ 00:01:05.580

BTS unit: 1:1
Channel No: 4 Name: DCCH
CFN: 167

Message Details:

#### CRLC Resume CNF

RLC LLA @ 00:01:05.580

BTS unit: 1:1
Channel No: 4 Name: DCCH
CFN: 167

Message Details:

#### CMAC Integrity Check Request

RRC MAC @ 00:01:05.590

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000001
Data:

[0]00 00 00 01
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:1 (RNC to UE)
Message Length (bits):336
Message:

[0]80 00 00 01 81 42 04 21
[8]00 40 7C 00 80 1E 22 00
[16]00 20 23 35 62 46 83 00
[24]BE 82 46 8A CF 04 60 BE
[32]82 24 46 68 89 40 60 1E
[40]82 40

#### CMAC Integrity Check Result

MAC RRC @ 00:01:05.590

Message Details:

Integrity Check Result:

MAC-I:11011110001010101000011011111100
Data:

[0]DE 2A 86 FC

#### CRLC_Resume_CNF

LLA RRC @ 00:01:05.590

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Resume_CNF:

cellId:-1

routingInfo:

rB_Identity:4

#### RRC_DATA_REQ: gmm:attachAccept

NAS RRC @ 00:01:05.590

Cell ID: -1

Message Details:

ATTACHACCEPT:

skipIndicator: 0000

gMMProtocolDiscriminator: 1000

msgType: 00000010

forceToStandby:

spare: 0

value: 000

attachResult:

spare: 0

result: 011

periodicRAupdateTimer:

unit: 111

value: 00000

spare: 0000

radioPrioSMS:

spare: 0

value: 100

rai:

plmn: 00F110

lac: 0001

rac: 01

ptmsiSignature:

iei: 00011001

value: AB1234

negReadyTimer: Omitted

allocatedPTMSI:

iei: 00011000

iel: 05

iDigit1: 1111

oddEvenInd: 0

typeOfId: 100

otherDigits: 12345678

msIdentity:

iei: 00100011

iel: 05

iDigit1: 1111

oddEvenInd: 0

typeOfId: 100

otherDigits: 11223344

gmmCause: Omitted

t3302Value: Omitted

cellNotification: Omitted

equivalentPLMN:

iei: 01001010

iel: 03

plmn1: 00F412

plmn2: Omitted

plmn3: Omitted

plmn4: Omitted

plmn5: Omitted

#### RLC_AM_DATA_REQ:downlinkDirectTransfer

RRC RLC @ 00:01:05.590

Channel No: 3 Name: DCCH

Message Details:

Opt1: 0

Opt2: 0

DL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode: 11011110001010101000011011111100

rrc_MessageSequenceNumber: 1

message:

downlinkDirectTransfer:

r3:

downlinkDirectTransfer_r3:

rrc_TransactionIdentifier: 0

cn_DomainIdentity: ps_domain_CN_DomainIdentity [enum=1]

nas_Message: 080203E00400F11000010119AB12341805F4123456782305F4112233444A0300F412

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]EF 15 43 7E 09 42 04 21
[8]00 40 7C 00 80 1E 22 00
[16]00 20 23 35 62 46 83 00
[24]BE 82 46 8A CF 04 60 BE
[32]82 24 46 68 89 40 60 1E
[40]82 40

#### MAC_DATA_REQ

RLC MAC @ 00:01:05.610

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 170

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 18 EF 15 43 7E 09 42
[8]04 21 00 40 7C 00 80 1E
[16]22 00

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:3
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]EF 15 43 7E 09 42 04 21
[8]00 40 7C 00 80 1E 22 00

#### MAC_DATA_REQ

RLC MAC @ 00:01:05.610

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 170

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 20 00 20 23 35 62 46
[8]83 00 BE 82 46 8A CF 04
[16]60 BE

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:4
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]00 20 23 35 62 46 83 00
[8]BE 82 46 8A CF 04 60 BE

#### MAC_DATA_REQ

RLC MAC @ 00:01:05.610

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 170

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 2D 15 FE 82 24 46 68
[8]89 40 60 1E 82 40 00 00
[16]00 00

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:5
Polling bit:1 (request a status report)
Length indicator 0 (octets):10
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (10 octets):

[0]82 24 46 68 89 40 60 1E
[8]82 40
Padding associated with length indicator 1 (4 octets):

[0]00 00 00 00

#### PHY_DATA_REQ

MAC PHY @ 00:01:05.620

BTS unit: 1:1
Channel No: 0 Name: FACH
CFN: 171

Message Details:

TFI:2
TB set size:336
TB size:168
TB set (raw, each TB word aligned):

[0]D0 00 12 80 18 EF 15 43
[8]7E 09 42 04 21 00 40 7C
[16]00 80 1E 22 00 00 D0 00
[24]12 80 20 00 20 23 35 62
[32]46 83 00 BE 82 46 8A CF
[40]04 60 BE 00

TB set (decoded):

TB 0:

TCTF:3
UEID type:C-RNTI
UEID:1
C/T:2
MAC SDU (144 bits):

[0]80 18 EF 15 43 7E 09 42
[8]04 21 00 40 7C 00 80 1E
[16]22 00

TB 1:

TCTF:3
UEID type:C-RNTI
UEID:1
C/T:2
MAC SDU (144 bits):

[0]80 20 00 20 23 35 62 46
[8]83 00 BE 82 46 8A CF 04
[16]60 BE

#### PHY_DATA_REQ

MAC PHY @ 00:01:05.630

BTS unit: 1:1
Channel No: 0 Name: FACH
CFN: 172

Message Details:

TFI:1
TB set size:168
TB size:168
TB set (raw):

[0]D0 00 12 80 2D 15 FE 82
[8]24 46 68 89 40 60 1E 82
[16]40 00 00 00 00 00

TB set (decoded):

TB 0:

TCTF:3
UEID type:C-RNTI
UEID:1
C/T:2
MAC SDU (144 bits):

[0]80 2D 15 FE 82 24 46 68
[8]89 40 60 1E 82 40 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:01:05.880

BTS unit: 1:1
Channel No: 0 Name: U_RACH
CFN: 177

Message Details:

TFI:0
TB set size:168
TB size:168
TB set (raw):

[0]50 00 12 02 00 60 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00 00 00

TB set (decoded):

TB 0:

TCTF:1
UEID type:C-RNTI
UEID:1
C/T:2
MAC SDU (144 bits):

[0]02 00 60 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### MAC_DATA_IND

MAC RLC @ 00:01:05.880

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 177

Message Details:

RLC PDU size (bits):142
RLC PDU (raw):

[0]02 00 60 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:6

#### PHY_DATA_IND

PHY MAC @ 00:01:05.940

BTS unit: 1:1
Channel No: 0 Name: U_RACH
CFN: 183

Message Details:

TFI:0
TB set size:168
TB size:168
TB set (raw):

[0]50 00 12 80 2D 15 FE D6
[8]F6 F7 1E 0E C8 00 84 01
[16]80 55 55 55 55 00

TB set (decoded):

TB 0:

TCTF:1
UEID type:C-RNTI
UEID:1
C/T:2
MAC SDU (144 bits):

[0]80 2D 15 FE D6 F6 F7 1E
[8]0E C8 00 84 01 80 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:01:05.940

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 183

Message Details:

RLC PDU size (bits):142
RLC PDU (raw):

[0]80 2D 15 FE D6 F6 F7 1E
[8]0E C8 00 84 01 80 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:5
Polling bit:1 (request a status report)
Length indicator 0 (octets):10
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (10 octets):

[0]D6 F6 F7 1E 0E C8 00 84
[8]01 80
Padding associated with length indicator 1 (4 octets):

[0]55 55 55 55

#### RLC_AM_DATA_IND: uplinkDirectTransfer

RLC RRC @ 00:01:05.950

Channel No: 3 Name: DCCH

Message Details:

UL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode: 10101101111011011110111000111100

rrc_MessageSequenceNumber: 1

message:

uplinkDirectTransfer:

cn_DomainIdentity: ps_domain_CN_DomainIdentity [enum=1]

nas_Message: 0803

measuredResultsOnRACH: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]D6 F6 F7 1E 0E C8 00 84
[8]01 80

#### RRC_DATA_IND: gmm:attachComplete

RRC NAS @ 00:01:05.950

Cell ID: -1

Message Details:

ATTACHCOMPLETE:

skipIndicator: 0000

gMMProtocolDiscriminator: 1000

msgType: 00000011

#### MAC_DATA_REQ

RLC MAC @ 00:01:05.950

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 204

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 60 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:6

#### CMAC Integrity Check Request

RRC MAC @ 00:01:05.950

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000001
Data:

[0]00 00 00 01
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:0 (UE to RNC)
Message Length (bits):80
Message:

[0]80 00 00 01 86 C8 00 84
[8]01 80

#### CMAC Integrity Check Result

MAC RRC @ 00:01:05.950

Message Details:

Integrity Check Result:

MAC-I:10101101111011011110111000111100
Data:

[0]AD ED EE 3C

#### PHY_DATA_REQ

MAC PHY @ 00:01:05.950

BTS unit: 1:1
Channel No: 0 Name: FACH
CFN: 204

Message Details:

TFI:1
TB set size:168
TB size:168
TB set (raw):

[0]D0 00 12 02 00 60 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00 00 00

TB set (decoded):

TB 0:

TCTF:3
UEID type:C-RNTI
UEID:1
C/T:2
MAC SDU (144 bits):

[0]02 00 60 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### CMAC Integrity Check Request

RRC MAC @ 00:01:06.970

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000001
Data:

[0]00 00 00 01
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:1 (RNC to UE)
Message Length (bits):56
Message:

[0]80 00 00 00 83 C0 00

#### CMAC Integrity Check Result

MAC RRC @ 00:01:06.970

Message Details:

Integrity Check Result:

MAC-I:10000001111010010001000100010101
Data:

[0]81 E9 11 15

#### RLC_UM_DATA_REQ

RRC LLA @ 00:01:06.970

Channel ID: Rb1
Cell ID: -1

Message Details:

RLC_UM_DATA_REQ:

cellId:-1

routingInfo:

rB_Identity:1

uM_message:

dL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode:00000000000000000000000000000000
rrc_MessageSequenceNumber:0

message: (DL_DCCH_MessageType)

rrcConnectionRelease:

r3:

rrcConnectionRelease_r3: (RRCConnectionRelease_r3_IEs)

rrc_TransactionIdentifier:0
n_308: Omit
releaseCause:normalEvent

rplmn_information: Omit

laterNonCriticalExtensions: Omit

specialLI:false

#### RLC_UM_DATA_REQ: rrcConnectionRelease

LLA RLC @ 00:01:06.970

Channel No: 1 Name: DCCH

Message Details:

DL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode: 10000001111010010001000100010101

rrc_MessageSequenceNumber: 1

message:

rrcConnectionRelease:

r3:

rrcConnectionRelease_r3:

rrc_TransactionIdentifier: 0

n_308: Omitted

releaseCause: normalEvent_ReleaseCause [enum=0]

rplmn_information: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]C0 F4 88 8A 8B C0 00

#### MAC_DATA_REQ

RLC MAC @ 00:01:06.980

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 51

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]01 0F FE C0 F4 88 8A 8B
[8]C0 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

Sequence number:0
Length indicator 0 (octets):7
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (7 octets):

[0]C0 F4 88 8A 8B C0 00
Padding associated with length indicator 1 (8 octets):

[0]00 00 00 00 00 00 00 00

#### PHY_DATA_REQ

MAC PHY @ 00:01:06.990

BTS unit: 1:1
Channel No: 0 Name: FACH
CFN: 52

Message Details:

TFI:1
TB set size:168
TB size:168
TB set (raw):

[0]D0 00 10 01 0F FE C0 F4
[8]88 8A 8B C0 00 00 00 00
[16]00 00 00 00 00 00

TB set (decoded):

TB 0:

TCTF:3
UEID type:C-RNTI
UEID:1
C/T:0
MAC SDU (144 bits):

[0]01 0F FE C0 F4 88 8A 8B
[8]C0 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:01:07.240

BTS unit: 1:1
Channel No: 0 Name: U_RACH
CFN: 57

Message Details:

TFI:0
TB set size:168
TB size:168
TB set (raw):

[0]50 00 11 80 25 0D FE 8E
[8]50 3A A3 94 40 55 55 55
[16]55 55 55 55 55 00

TB set (decoded):

TB 0:

TCTF:1
UEID type:C-RNTI
UEID:1
C/T:1
MAC SDU (144 bits):

[0]80 25 0D FE 8E 50 3A A3
[8]94 40 55 55 55 55 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:01:07.240

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 57

Message Details:

RLC PDU size (bits):142
RLC PDU (raw):

[0]80 25 0D FE 8E 50 3A A3
[8]94 40 55 55 55 55 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:4
Polling bit:1 (request a status report)
Length indicator 0 (octets):6
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (6 octets):

[0]8E 50 3A A3 94 40
Padding associated with length indicator 1 (8 octets):

[0]55 55 55 55 55 55 55 55

#### MAC_DATA_REQ

RLC MAC @ 00:01:07.250

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 78

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 50 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:5

#### PHY_DATA_REQ

MAC PHY @ 00:01:07.250

BTS unit: 1:1
Channel No: 0 Name: FACH
CFN: 78

Message Details:

TFI:1
TB set size:168
TB size:168
TB set (raw):

[0]D0 00 11 02 00 50 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00 00 00

TB set (decoded):

TB 0:

TCTF:3
UEID type:C-RNTI
UEID:1
C/T:1
MAC SDU (144 bits):

[0]02 00 50 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### CMAC Integrity Check Request

RRC MAC @ 00:01:07.260

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000010
Data:

[0]00 00 00 02
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:0 (UE to RNC)
Message Length (bits):48
Message:

[0]80 00 00 01 04 40

#### RLC_AM_DATA_IND: rrcConnectionReleaseComplete

RLC LLA @ 00:01:07.260

Channel No: 2 Name: DCCH

Message Details:

UL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode: 00011100101000000111010101000111

rrc_MessageSequenceNumber: 2

message:

rrcConnectionReleaseComplete:

rrc_TransactionIdentifier: 0

errorIndication: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]8E 50 3A A3 94 40

#### CMAC Integrity Check Result

MAC RRC @ 00:01:07.260

Message Details:

Integrity Check Result:

MAC-I:00011100101000000111010101000111
Data:

[0]1C A0 75 47

#### RLC_AM_DATA_IND

LLA RRC @ 00:01:07.260

Channel ID: Rb2
Cell ID: -1

Message Details:

RLC_AM_DATA_IND:

cellId:-1

routingInfo:

rB_Identity:2

integrityResult:

integrityUsed (IntegrityStatus):i_pass

aM_message:

uL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode:00011100101000000111010101000111
rrc_MessageSequenceNumber:2

message: (UL_DCCH_MessageType)

rrcConnectionReleaseComplete:

rrc_TransactionIdentifier:0

errorIndication: (FailureCauseWithProtErr) Omit

laterNonCriticalExtensions: Omit

#### CRLC_Config_REQ

RRC LLA @ 00:01:08.280

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:1

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC_Config_CNF

LLA RRC @ 00:01:08.290

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:1

#### CRLC_Config_REQ

RRC LLA @ 00:01:08.290

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:2

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC UM Channel Release REQ

LLA RLC @ 00:01:08.290

BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 182

Message Details:

#### CRLC UM Channel Release CNF

RLC LLA @ 00:01:08.290

BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 182

Message Details:

#### CRLC AM Channel Release REQ

LLA RLC @ 00:01:08.300

BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 183

Message Details:

#### CRLC AM Channel Release CNF

RLC LLA @ 00:01:08.300

BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 183

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:01:08.310

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:2

#### CRLC_Config_REQ

RRC LLA @ 00:01:08.310

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:3

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC AM Channel Release REQ

LLA RLC @ 00:01:08.320

BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 185

Message Details:

#### CRLC AM Channel Release CNF

RLC LLA @ 00:01:08.320

BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 185

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:01:08.330

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:3

#### CRLC_Config_REQ

RRC LLA @ 00:01:08.330

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:4

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC AM Channel Release REQ

LLA RLC @ 00:01:08.330

BTS unit: 1:1
Channel No: 4 Name: DCCH
CFN: 186

Message Details:

#### CRLC AM Channel Release CNF

RLC LLA @ 00:01:08.330

BTS unit: 1:1
Channel No: 4 Name: DCCH
CFN: 186

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:01:08.340

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:4

#### CRLC_Config_REQ

RRC LLA @ 00:01:08.340

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:1

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode)

dl_UM_RLC_Mode:

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):136

dl_RLCModeInfo: (UL_RLC_Mode)

ul_UM_RLC_Mode:

transmissionRLC_Discard:

timerBasedNoExplicit (NoExplicitDiscard):dt100

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity):1
dLlogicalChannelIdentity (LogicalChannelIdentity):1
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC UM Channel Establish REQ

LLA RLC @ 00:01:08.350

BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 188

Message Details:

Configuration Parameters:

PU Size In Bits:136

#### CRLC UM Channel Establish CNF

RLC LLA @ 00:01:08.350

BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 188

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:01:08.360

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:1

#### CRLC_Config_REQ

RRC LLA @ 00:01:08.360

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:2

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode)

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):128

dl_RLCModeInfo: (UL_RLC_Mode)

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp400
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity):2
dLlogicalChannelIdentity (LogicalChannelIdentity):2
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC_Config_CNF

LLA RRC @ 00:01:08.370

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:2

#### CRLC_Config_REQ

RRC LLA @ 00:01:08.370

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:3

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode)

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):128

dl_RLCModeInfo: (UL_RLC_Mode)

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp400
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity):3
dLlogicalChannelIdentity (LogicalChannelIdentity):3
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC AM Channel Establish REQ

LLA RLC @ 00:01:08.370

BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 190

Message Details:

Configuration Parameters:

PU Size In Bits:128

Timer Parameters:

Poll (ms):400
Poll Prohibit (ms):0
EPC (ms):0
Discard (ms):0
Poll Periodic (ms):0
Status Prohibit (ms):0
Status Periodic (ms):0
Reset (ms):500
MRW (ms):0

Protocol Parameters:

Max Dat:15
Poll PU:0
Poll SDU:1
Poll Window:99
Max Reset:1
Tx Window Size:32
Rx Window Size:32
Max MRW:0
SDU Discard Mode:No discard

Polling Triggers:

Last PU In Buffer:On
Last PU In Retransmission Buffer:On
Poll Timer:On
Every Poll-PU PU:Off
Every Poll-SDU SDU:On
Poll-Window Percent Of Transmission Buffer:On
Timer Based:Off

Status Triggers:

Missing PU:On
Timer Based:Off
EPC Mechanism:Off

#### CRLC AM Channel Establish CNF

RLC LLA @ 00:01:08.370

BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 190

Message Details:

#### CRLC AM Channel Establish REQ

LLA RLC @ 00:01:08.380

BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 191

Message Details:

Configuration Parameters:

PU Size In Bits:128

Timer Parameters:

Poll (ms):400
Poll Prohibit (ms):0
EPC (ms):0
Discard (ms):0
Poll Periodic (ms):0
Status Prohibit (ms):0
Status Periodic (ms):0
Reset (ms):500
MRW (ms):0

Protocol Parameters:

Max Dat:15
Poll PU:0
Poll SDU:1
Poll Window:99
Max Reset:1
Tx Window Size:32
Rx Window Size:32
Max MRW:0
SDU Discard Mode:No discard

Polling Triggers:

Last PU In Buffer:On
Last PU In Retransmission Buffer:On
Poll Timer:On
Every Poll-PU PU:Off
Every Poll-SDU SDU:On
Poll-Window Percent Of Transmission Buffer:On
Timer Based:Off

Status Triggers:

Missing PU:On
Timer Based:Off
EPC Mechanism:Off

#### CRLC AM Channel Establish CNF

RLC LLA @ 00:01:08.380

BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 191

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:01:08.390

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:3

#### CRLC_Config_REQ

RRC LLA @ 00:01:08.390

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:4

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode)

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):128

dl_RLCModeInfo: (UL_RLC_Mode)

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp400
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity):4
dLlogicalChannelIdentity (LogicalChannelIdentity):4
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC_Config_CNF

LLA RRC @ 00:01:08.400

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:4

#### CPHY_Cell_Config_REQ

RRC LLA @ 00:01:08.400

Cell ID: 3

Message Details:

CPHY_Cell_Config_REQ:

cellId:3
tcell:321
sfnOffset:3000

frequencyInfo:

modeSpecificInfo:

fdd: (FrequencyInfoFDD)

uarfcn_UL (UARFCN):9663
uarfcn_DL (UARFCN):10613

primaryScramblingCode_SS:200

cellTxPowerLevel:

defaultCellTxPowerLvl:

dLTxAttenuationLevel:2

#### CRLC AM Channel Establish REQ

LLA RLC @ 00:01:08.400

BTS unit: 1:1
Channel No: 4 Name: DCCH
CFN: 193

Message Details:

Configuration Parameters:

PU Size In Bits:128

Timer Parameters:

Poll (ms):400
Poll Prohibit (ms):0
EPC (ms):0
Discard (ms):0
Poll Periodic (ms):0
Status Prohibit (ms):0
Status Periodic (ms):0
Reset (ms):500
MRW (ms):0

Protocol Parameters:

Max Dat:15
Poll PU:0
Poll SDU:1
Poll Window:99
Max Reset:1
Tx Window Size:32
Rx Window Size:32
Max MRW:0
SDU Discard Mode:No discard

Polling Triggers:

Last PU In Buffer:On
Last PU In Retransmission Buffer:On
Poll Timer:On
Every Poll-PU PU:Off
Every Poll-SDU SDU:On
Poll-Window Percent Of Transmission Buffer:On
Timer Based:Off

Status Triggers:

Missing PU:On
Timer Based:Off
EPC Mechanism:Off

#### CRLC AM Channel Establish CNF

RLC LLA @ 00:01:08.400

BTS unit: 1:1
Channel No: 4 Name: DCCH
CFN: 193

Message Details:

#### CPHY BTS Frequency REQ

LLA PHY @ 00:01:08.380

BTS unit: 2:1
CFN: 191

Message Details:

Configuration Parameters:

Down Link Frequency:2122600000
Up Link Frequency:1932600000

#### CPHY BTS Frequency CNF

PHY LLA @ 00:01:08.380

BTS unit: 2:1
CFN: 191

Message Details:

#### CPHY Radio Link Setup REQ

LLA PHY @ 00:01:08.400

BTS unit: 2:1
Channel No: 0 Name: P_CPICH
CFN: 193

Message Details:

Configuration Parameters:

Channel Offset:7680
Scrambling Code:3200
Symbol Rate:15k
Channelization Code:0
Adjust Time:0
Power in dBm:-42
Tx Diversity:Off
NumOfDpdch:0

#### CPHY Radio Link Setup CNF

PHY LLA @ 00:01:08.400

BTS unit: 2:1
Channel No: 0 Name: P_CPICH
CFN: 193

Message Details:

#### CPHY Radio Link Setup REQ

LLA PHY @ 00:01:08.420

BTS unit: 2:1
Channel No: 0 Name: P_SCH
CFN: 195

Message Details:

Configuration Parameters:

Channel Offset:7680
Adjust Time:0
Power in dBm:-47
Tx Diversity:Off
NumOfDpdch:0

#### CPHY Radio Link Setup CNF

PHY LLA @ 00:01:08.420

BTS unit: 2:1
Channel No: 0 Name: P_SCH
CFN: 195

Message Details:

#### CPHY_Cell_Config_CNF

LLA RRC @ 00:01:08.440

Cell ID: 3

Message Details:

CPHY_Cell_Config_CNF:

cellId:3

#### CPHY_RL_Setup_REQ

RRC LLA @ 00:01:08.440

Channel ID: P-CPICH
Cell ID: 3

Message Details:

CPHY_RL_Setup_REQ:

cellId:3

routingInfo:

physicalChannelIdentity:0

ratType:fdd

setupMessage: (CphyRlSetupReq)

physicalChannelInfo:

primaryCPICHInfo:

dl_TxPower_PCPICH:-60
txdiversityIndicator:false

#### CPHY Radio Link Setup REQ

LLA PHY @ 00:01:08.440

BTS unit: 2:1
Channel No: 0 Name: S_SCH
CFN: 197

Message Details:

Configuration Parameters:

Channel Offset:7680
Adjust Time:0
Power in dBm:-47
Tx Diversity:Off
NumOfDpdch:0

#### CPHY Radio Link Setup CNF

PHY LLA @ 00:01:08.440

BTS unit: 2:1
Channel No: 0 Name: S_SCH
CFN: 197

Message Details:

#### CPHY_RL_Setup_CNF

LLA RRC @ 00:01:08.450

Channel ID: P-CPICH
Cell ID: 3

Message Details:

CPHY_RL_Setup_CNF:

cellId:3

routingInfo:

physicalChannelIdentity:0

#### CPHY_RL_Setup_REQ

RRC LLA @ 00:01:08.450

Channel ID: P-SCH
Cell ID: 3

Message Details:

CPHY_RL_Setup_REQ:

cellId:3

routingInfo:

physicalChannelIdentity:1

ratType:fdd

setupMessage: (CphyRlSetupReq)

physicalChannelInfo:

primarySCHInfo:

tstdIndicator:false
dl_TxPower:-5

#### CPHY Radio Link Setup REQ

LLA PHY @ 00:01:08.450

BTS unit: 2:1
Channel No: 0 Name: P_CCPCH
CFN: 198

Message Details:

Configuration Parameters:

Channel Offset:7680
SFN Offset:0
Scrambling Code:3200
Symbol Rate:15k
Channelization Code:1
Adjust Time:0
Power in dBm:-44
Tx Diversity:Off
NumOfDpdch:1

#### CPHY Radio Link Setup CNF

PHY LLA @ 00:01:08.450

BTS unit: 2:1
Channel No: 0 Name: P_CCPCH
CFN: 198

Message Details:

#### CPHY_RL_Setup_CNF

LLA RRC @ 00:01:08.470

Channel ID: P-SCH
Cell ID: 3

Message Details:

CPHY_RL_Setup_CNF:

cellId:3

routingInfo:

physicalChannelIdentity:1

#### CPHY_RL_Setup_REQ

RRC LLA @ 00:01:08.470

Channel ID: S-SCH
Cell ID: 3

Message Details:

CPHY_RL_Setup_REQ:

cellId:3

routingInfo:

physicalChannelIdentity:2

ratType:fdd

setupMessage: (CphyRlSetupReq)

physicalChannelInfo:

secondarySCHInfo:

tstdIndicator:false
dl_TxPower:-5

#### CPHY Transport Channel Configuration REQ

LLA PHY @ 00:01:08.470

BTS unit: 2:1
Channel No: 0 Name: P_CCPCH
CFN: 200

Message Details:

Configuration Parameters:

DTX Position:Flexible
Second Interleave:On
Puncture Limit:0
CCTrCH Length:270
Number Of Transport Channels:1

Transport Channels:

Item Number 0:

Transport Channel Parameters:

Transport Channel:

Name:BCH
Identity:0

TTI (ms):20
EP Type:1/2 Rate Convolutional Coding
CRC Size:16
RM Attribute:1
First Interleave:On
Number Of Transport Formats:2

Transport Format Set:

Transport Format 0:

Number Of Transport Blocks:0
Transport Block Size In Bits:0

Transport Format 1:

Number Of Transport Blocks:1
Transport Block Size In Bits:246

RM Maximum Length:540

Transport Format Combination Set:

Number Of Transport Format Combinations:2

Transport Format Combinations 0:

Transport Format:0

Transport Format Combinations 1:

Transport Format:1

#### CPHY Transport Channel Configuration CNF

PHY LLA @ 00:01:08.470

BTS unit: 2:1
Channel No: 0 Name: P_CCPCH
CFN: 200

Message Details:

#### CPHY_RL_Setup_CNF

LLA RRC @ 00:01:08.480

Channel ID: S-SCH
Cell ID: 3

Message Details:

CPHY_RL_Setup_CNF:

cellId:3

routingInfo:

physicalChannelIdentity:2

#### CPHY_RL_Setup_REQ

RRC LLA @ 00:01:08.480

Channel ID: P-CCPCH
Cell ID: 3

Message Details:

CPHY_RL_Setup_REQ:

cellId:3

routingInfo:

physicalChannelIdentity:4

ratType:fdd

setupMessage: (CphyRlSetupReq)

physicalChannelInfo:

primaryCCPCHInfo:

sttd_Indicator:false
dl_TxPower:-2

#### CMAC Configuration REQ

LLA MAC @ 00:01:08.490

BTS unit: 2:1
Channel No: 0 Name: P_CCPCH
CFN: 202

Message Details:

Configuration Parameters:

Number Of Transport Channels:1

Transport Channels:

Item Number 0:

Transport Channel Parameters:

Transport Channel:

Name:BCH
Identity:0

TTI (ms):20
EP Type:1/2 Rate Convolutional Coding
CRC Size:16
RM Attribute:1
First Interleave:On
Number Of Transport Formats:2

Transport Format Set:

Transport Format 0:

Number Of Transport Blocks:0
Transport Block Size In Bits:0

Transport Format 1:

Number Of Transport Blocks:1
Transport Block Size In Bits:246

Number Of Logical Channels:1

Logical Channels:

Item Number 0:

Logical Channel:

Name:BCCH
Identity:0

Priority:1
CT Length:0
CT Value:0
TCTF Length:0
TCTF Value:0
UE ID Type:Not used
UE ID:0

Active Flag:1

Transport Format Combination Set:

Number Of Transport Format Combinations:2

Transport Format Combinations 0:

Transport Format:0

Transport Format Combinations 1:

Transport Format:1

#### CMAC Configuration CNF

MAC LLA @ 00:01:08.490

BTS unit: 2:1
Channel No: 0 Name: P_CCPCH
CFN: 202

Message Details:

#### CPHY_RL_Setup_CNF

LLA RRC @ 00:01:08.500

Channel ID: P-CCPCH
Cell ID: 3

Message Details:

CPHY_RL_Setup_CNF:

cellId:3

routingInfo:

physicalChannelIdentity:4

#### CPHY_TrCH_Config_REQ

RRC LLA @ 00:01:08.500

Channel ID: P-CCPCH
Cell ID: 3

Message Details:

CPHY_TrCH_Config_REQ:

cellId:3

routingInfo:

physicalChannelIdentity:4

ratType:fdd

trchConfigType:

nonDch:

configMessage: (CphyTrchConfigReq)

activationTime: (SS_ActivationTime)

activateNow:

ulconnectedTrCHList: Omit

ulTFCS: (TFCS) Omit

dlconnectedTrCHList:

:

trchid (TransportChannelIdentity):11
dl_TransportChannelType (SS_DL_TransportChannelType):bch

transportChannelInfo: (CommonOrDedicatedTFS)

tti:

tti20: (CommonOrDedicatedTF_InfoList)

CommonOrDedicatedTF_Info:

tb_Size:246

numberOfTbSizeList:

NumberOfTransportBlocks:

one:

logicalChannelList:

configured:

semistaticTF_Information:

channelCodingType:

convolutional (CodingRate):half

rateMatchingAttribute:1
crc_Size:crc16

dlTFCS: (TFCS)

normalTFCI_Signalling: (ExplicitTFCS_Configuration)

complete: (TFCS_ReconfAdd)

ctfcSize:

ctfc2Bit:

:

ctfc2:0

powerOffsetInformation:

gainFactorInformation:

signalledGainFactors:

modeSpecificInfo:

fdd:

gainFactorBetaC (GainFactor):11

gainFactorBetaD (GainFactor):15
referenceTFC_ID:0

powerOffsetPp_m: Omit

#### CPHY_TrCH_Config_CNF

LLA RRC @ 00:01:08.510

Channel ID: P-CCPCH
Cell ID: 3

Message Details:

CPHY_TrCH_Config_CNF:

cellId:3

routingInfo:

physicalChannelIdentity:4

#### CMAC_Config_REQ

RRC LLA @ 00:01:08.510

Channel ID: P-CCPCH
Cell ID: 3

Message Details:

CMAC_Config_REQ:

cellId:3

routingInfo:

physicalChannelIdentity:4

ratType:fdd

configMessage:

setup: (CmacConfigReq)

activationTime: (SS_ActivationTime)

activateNow:

uE_Info:

u_RNTI: Omit

c_RNTI: Omit

trCHInfo:

ulconnectedTrCHList: Omit

ulTFCS: (TFCS) Omit

dlconnectedTrCHList:

:

trchid (TransportChannelIdentity):11

transportChannelInfo: (CommonOrDedicatedTFS)

tti:

tti20: (CommonOrDedicatedTF_InfoList)

CommonOrDedicatedTF_Info:

tb_Size:246

numberOfTbSizeList:

NumberOfTransportBlocks:

one:

logicalChannelList:

configured:

semistaticTF_Information:

channelCodingType:

convolutional (CodingRate):half

rateMatchingAttribute:1
crc_Size:crc16

dlTFCS: (TFCS)

normalTFCI_Signalling: (ExplicitTFCS_Configuration)

complete: (TFCS_ReconfAdd)

ctfcSize:

ctfc2Bit:

:

ctfc2:0

powerOffsetInformation:

gainFactorInformation:

signalledGainFactors:

modeSpecificInfo:

fdd:

gainFactorBetaC (GainFactor):11

gainFactorBetaD (GainFactor):15
referenceTFC_ID:0

powerOffsetPp_m: Omit

trCH_LogCHMapping: (TrCH_LogCHMappingList1)

ulconnectedTrCHList: Omit

dlconnectedTrCHList:

:

trchid (TransportChannelIdentity):11

trCH_LogCHMappingList:

TrCH_LogicalChannelMapping:

logicalChannel_Mapping:

dl_LogicalChannelMapping: (SS_DL_LogicalChannelMapping)

macHeaderManipulation (MAC_HeaderManipulation):normalMacHeader
dl_TransportChannelType (SS_DL_TransportChannelType):bch
logicalChannelIdentity:1
logicalChannelType:bCCH

rlc_SizeList:

configured:

mac_LogicalChannelPriority:1

rB_Identity:-1
cn_DomainIdentity: Omit

#### CPHY Radio Link Setup REQ

LLA PHY @ 00:01:08.520

BTS unit: 2:1
Channel No: 0 Name: S_CCPCH
CFN: 205

Message Details:

Configuration Parameters:

Channel Offset:7680
Scrambling Code:3200
Symbol Rate:60k
Channelization Code:1
Adjust Time:0
Power in dBm:-44
Tx Diversity:Off
Slot Format:8
NumOfDpdch:1

#### CPHY Radio Link Setup CNF

PHY LLA @ 00:01:08.520

BTS unit: 2:1
Channel No: 0 Name: S_CCPCH
CFN: 205

Message Details:

#### CMAC_Config_CNF

LLA RRC @ 00:01:08.540

Channel ID: P-CCPCH
Cell ID: 3

Message Details:

CMAC_Config_CNF:

cellId:3

routingInfo:

physicalChannelIdentity:4

#### CPHY_RL_Setup_REQ

RRC LLA @ 00:01:08.540

Channel ID: S-CCPCH#1
Cell ID: 3

Message Details:

CPHY_RL_Setup_REQ:

cellId:3

routingInfo:

physicalChannelIdentity:5

ratType:fdd

setupMessage: (CphyRlSetupReq)

physicalChannelInfo:

secondaryCCPCHInfo:

scramblingCode:0

dl_ChannelizationCode: (SF256_AndCodeNumber)

sf64:1

sCCPCHSlotFormat:8
timingOffset:0
positionFixedOrFlexible:flexible
sttd_Indicator:false
dl_TxPower:-2
powerOffsetOfTFCI_PO1:6
powerOffsetOfPILOT_PO3:6

#### CPHY Transport Channel Configuration REQ

LLA PHY @ 00:01:08.550

BTS unit: 2:1
Channel No: 0 Name: S_CCPCH
CFN: 208

Message Details:

Configuration Parameters:

DTX Position:Flexible
Second Interleave:On
Puncture Limit:100
CCTrCH Length:1080
Number Of Transport Channels:3

Transport Channels:

Item Number 0:

Transport Channel Parameters:

Transport Channel:

Name:PCH
Identity:0

TTI (ms):10
EP Type:1/2 Rate Convolutional Coding
CRC Size:16
RM Attribute:230
First Interleave:On
Number Of Transport Formats:2

Transport Format Set:

Transport Format 0:

Number Of Transport Blocks:0
Transport Block Size In Bits:240

Transport Format 1:

Number Of Transport Blocks:1
Transport Block Size In Bits:240

RM Maximum Length:457

Item Number 1:

Transport Channel Parameters:

Transport Channel:

Name:FACH
Identity:0

TTI (ms):10
EP Type:1/2 Rate Convolutional Coding
CRC Size:16
RM Attribute:220
First Interleave:On
Number Of Transport Formats:3

Transport Format Set:

Transport Format 0:

Number Of Transport Blocks:0
Transport Block Size In Bits:168

Transport Format 1:

Number Of Transport Blocks:1
Transport Block Size In Bits:168

Transport Format 2:

Number Of Transport Blocks:2
Transport Block Size In Bits:168

RM Maximum Length:623

Item Number 2:

Transport Channel Parameters:

Transport Channel:

Name:FACH
Identity:1

TTI (ms):10
EP Type:Turbo Coding
CRC Size:16
RM Attribute:130
First Interleave:On
Number Of Transport Formats:2

Transport Format Set:

Transport Format 0:

Number Of Transport Blocks:0
Transport Block Size In Bits:360

Transport Format 1:

Number Of Transport Blocks:1
Transport Block Size In Bits:360

RM Maximum Length:558

Transport Format Combination Set:

Number Of Transport Format Combinations:8

Transport Format Combinations 0:

Transport Format:0
Transport Format:0
Transport Format:0

Transport Format Combinations 1:

Transport Format:1
Transport Format:0
Transport Format:0

Transport Format Combinations 2:

Transport Format:0
Transport Format:1
Transport Format:0

Transport Format Combinations 3:

Transport Format:1
Transport Format:1
Transport Format:0

Transport Format Combinations 4:

Transport Format:0
Transport Format:2
Transport Format:0

Transport Format Combinations 5:

Transport Format:1
Transport Format:2
Transport Format:0

Transport Format Combinations 6:

Transport Format:0
Transport Format:0
Transport Format:1

Transport Format Combinations 7:

Transport Format:0
Transport Format:1
Transport Format:1

#### CPHY Transport Channel Configuration CNF

PHY LLA @ 00:01:08.550

BTS unit: 2:1
Channel No: 0 Name: S_CCPCH
CFN: 208

Message Details:

#### CPHY_RL_Setup_CNF

LLA RRC @ 00:01:08.580

Channel ID: S-CCPCH#1
Cell ID: 3

Message Details:

CPHY_RL_Setup_CNF:

cellId:3

routingInfo:

physicalChannelIdentity:5

#### CPHY_TrCH_Config_REQ

RRC LLA @ 00:01:08.580

Channel ID: S-CCPCH#1
Cell ID: 3

Message Details:

CPHY_TrCH_Config_REQ:

cellId:3

routingInfo:

physicalChannelIdentity:5

ratType:fdd

trchConfigType:

nonDch:

configMessage: (CphyTrchConfigReq)

activationTime: (SS_ActivationTime)

activateNow:

ulconnectedTrCHList: Omit

ulTFCS: (TFCS) Omit

dlconnectedTrCHList:

:

trchid (TransportChannelIdentity):12
dl_TransportChannelType (SS_DL_TransportChannelType):pch

transportChannelInfo: (CommonOrDedicatedTFS)

tti:

tti10: (CommonOrDedicatedTF_InfoList)

CommonOrDedicatedTF_Info:

tb_Size:240

numberOfTbSizeList:

NumberOfTransportBlocks:

zero:

NumberOfTransportBlocks:

one:

logicalChannelList:

allSizes:

semistaticTF_Information:

channelCodingType:

convolutional (CodingRate):half

rateMatchingAttribute:230
crc_Size:crc16

:

trchid (TransportChannelIdentity):13
dl_TransportChannelType (SS_DL_TransportChannelType):fach

transportChannelInfo: (CommonOrDedicatedTFS)

tti:

tti10: (CommonOrDedicatedTF_InfoList)

CommonOrDedicatedTF_Info:

tb_Size:168

numberOfTbSizeList:

NumberOfTransportBlocks:

zero:

NumberOfTransportBlocks:

one:

NumberOfTransportBlocks:

small:2

logicalChannelList:

allSizes:

semistaticTF_Information:

channelCodingType:

convolutional (CodingRate):half

rateMatchingAttribute:220
crc_Size:crc16

:

trchid (TransportChannelIdentity):14
dl_TransportChannelType (SS_DL_TransportChannelType):fach

transportChannelInfo: (CommonOrDedicatedTFS)

tti:

tti10: (CommonOrDedicatedTF_InfoList)

CommonOrDedicatedTF_Info:

tb_Size:360

numberOfTbSizeList:

NumberOfTransportBlocks:

zero:

NumberOfTransportBlocks:

one:

logicalChannelList:

allSizes:

semistaticTF_Information:

channelCodingType:

turbo:

rateMatchingAttribute:130
crc_Size:crc16

dlTFCS: (TFCS)

normalTFCI_Signalling: (ExplicitTFCS_Configuration)

complete: (TFCS_ReconfAdd)

ctfcSize:

ctfc4Bit:

:

ctfc4:0

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:1

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:2

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:3

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:4

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:5

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:6

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:8

powerOffsetInformation:

gainFactorInformation:

signalledGainFactors:

modeSpecificInfo:

fdd:

gainFactorBetaC (GainFactor):11

gainFactorBetaD (GainFactor):15
referenceTFC_ID:0

powerOffsetPp_m: Omit

#### CPHY Radio Link Setup REQ

LLA PHY @ 00:01:08.590

BTS unit: 2:1
Channel No: 0 Name: PICH
CFN: 212

Message Details:

Configuration Parameters:

Channel Offset:0
Scrambling Code:3200
Symbol Rate:15k
Channelization Code:2
Adjust Time:0
Power in dBm:-47
Tx Diversity:Off
NumOfDpdch:0
Np:18

#### CPHY Radio Link Setup CNF

PHY LLA @ 00:01:08.590

BTS unit: 2:1
Channel No: 0 Name: PICH
CFN: 212

Message Details:

#### CPHY_TrCH_Config_CNF

LLA RRC @ 00:01:08.610

Channel ID: S-CCPCH#1
Cell ID: 3

Message Details:

CPHY_TrCH_Config_CNF:

cellId:3

routingInfo:

physicalChannelIdentity:5

#### CMAC_Config_REQ

RRC LLA @ 00:01:08.610

Channel ID: S-CCPCH#1
Cell ID: 3

Message Details:

CMAC_Config_REQ:

cellId:3

routingInfo:

physicalChannelIdentity:5

ratType:fdd

configMessage:

setup: (CmacConfigReq)

activationTime: (SS_ActivationTime)

activateNow:

uE_Info:

u_RNTI: Omit

c_RNTI: Omit

trCHInfo:

ulconnectedTrCHList: Omit

ulTFCS: (TFCS) Omit

dlconnectedTrCHList:

:

trchid (TransportChannelIdentity):12

transportChannelInfo: (CommonOrDedicatedTFS)

tti:

tti10: (CommonOrDedicatedTF_InfoList)

CommonOrDedicatedTF_Info:

tb_Size:240

numberOfTbSizeList:

NumberOfTransportBlocks:

zero:

NumberOfTransportBlocks:

one:

logicalChannelList:

allSizes:

semistaticTF_Information:

channelCodingType:

convolutional (CodingRate):half

rateMatchingAttribute:230
crc_Size:crc16

:

trchid (TransportChannelIdentity):13

transportChannelInfo: (CommonOrDedicatedTFS)

tti:

tti10: (CommonOrDedicatedTF_InfoList)

CommonOrDedicatedTF_Info:

tb_Size:168

numberOfTbSizeList:

NumberOfTransportBlocks:

zero:

NumberOfTransportBlocks:

one:

NumberOfTransportBlocks:

small:2

logicalChannelList:

allSizes:

semistaticTF_Information:

channelCodingType:

convolutional (CodingRate):half

rateMatchingAttribute:220
crc_Size:crc16

:

trchid (TransportChannelIdentity):14

transportChannelInfo: (CommonOrDedicatedTFS)

tti:

tti10: (CommonOrDedicatedTF_InfoList)

CommonOrDedicatedTF_Info:

tb_Size:360

numberOfTbSizeList:

NumberOfTransportBlocks:

zero:

NumberOfTransportBlocks:

one:

logicalChannelList:

allSizes:

semistaticTF_Information:

channelCodingType:

turbo:

rateMatchingAttribute:130
crc_Size:crc16

dlTFCS: (TFCS)

normalTFCI_Signalling: (ExplicitTFCS_Configuration)

complete: (TFCS_ReconfAdd)

ctfcSize:

ctfc4Bit:

:

ctfc4:0

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:1

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:2

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:3

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:4

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:5

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:6

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:8

powerOffsetInformation:

gainFactorInformation:

signalledGainFactors:

modeSpecificInfo:

fdd:

gainFactorBetaC (GainFactor):11

gainFactorBetaD (GainFactor):15
referenceTFC_ID:0

powerOffsetPp_m: Omit

trCH_LogCHMapping: (TrCH_LogCHMappingList1)

ulconnectedTrCHList: Omit

dlconnectedTrCHList:

:

trchid (TransportChannelIdentity):12

trCH_LogCHMappingList:

TrCH_LogicalChannelMapping:

logicalChannel_Mapping:

dl_LogicalChannelMapping: (SS_DL_LogicalChannelMapping)

macHeaderManipulation (MAC_HeaderManipulation):normalMacHeader
dl_TransportChannelType (SS_DL_TransportChannelType):pch
logicalChannelIdentity:1
logicalChannelType:pCCH

rlc_SizeList:

configured:

mac_LogicalChannelPriority:1

rB_Identity:-2
cn_DomainIdentity: Omit

:

trchid (TransportChannelIdentity):13

trCH_LogCHMappingList:

TrCH_LogicalChannelMapping:

logicalChannel_Mapping:

dl_LogicalChannelMapping: (SS_DL_LogicalChannelMapping)

macHeaderManipulation (MAC_HeaderManipulation):normalMacHeader
dl_TransportChannelType (SS_DL_TransportChannelType):fach
logicalChannelIdentity:5
logicalChannelType:cCCH

rlc_SizeList:

configured:

mac_LogicalChannelPriority:1

rB_Identity:0
cn_DomainIdentity: Omit

#### CPHY Radio Link Setup REQ

LLA PHY @ 00:01:08.610

BTS unit: 2:1
Channel No: 0 Name: AICH
CFN: 214

Message Details:

Configuration Parameters:

Channel Offset:7680
Scrambling Code:3200
Symbol Rate:15k
Channelization Code:3
Adjust Time:0
Power in dBm:-47
Tx Diversity:Off
AICH Transmission Timing:3 Access Slots
AICH Polarity:Positive
NumOfDpdch:0

#### CPHY Radio Link Setup CNF

PHY LLA @ 00:01:08.610

BTS unit: 2:1
Channel No: 0 Name: AICH
CFN: 214

Message Details:

#### CMAC_Config_CNF

LLA RRC @ 00:01:08.620

Channel ID: S-CCPCH#1
Cell ID: 3

Message Details:

CMAC_Config_CNF:

cellId:3

routingInfo:

physicalChannelIdentity:5

#### CPHY_RL_Setup_REQ

RRC LLA @ 00:01:08.620

Channel ID: PICH#1
Cell ID: 3

Message Details:

CPHY_RL_Setup_REQ:

cellId:3

routingInfo:

physicalChannelIdentity:6

ratType:fdd

setupMessage: (CphyRlSetupReq)

physicalChannelInfo:

pICHInfo:

pichinfo: (PICH_Info)

fdd:

channelisationCode256:2
pi_CountPerFrame:e18
sttd_Indicator:false

dl_TxPower (PICH_PowerOffset):-5
sccpchId_associated:5

#### CPHY_RL_Setup_CNF

LLA RRC @ 00:01:08.640

Channel ID: PICH#1
Cell ID: 3

Message Details:

CPHY_RL_Setup_CNF:

cellId:3

routingInfo:

physicalChannelIdentity:6

#### CPHY_RL_Setup_REQ

RRC LLA @ 00:01:08.640

Channel ID: AICH#1
Cell ID: 3

Message Details:

CPHY_RL_Setup_REQ:

cellId:3

routingInfo:

physicalChannelIdentity:7

ratType:fdd

setupMessage: (CphyRlSetupReq)

physicalChannelInfo:

aICHInfo:

aichinfo: (AICH_Info)

channelisationCode256:3
sttd_Indicator:false
aich_TransmissionTiming:e0

dl_TxPower (AICH_PowerOffset):-5

#### CPHY Radio Link Setup REQ

LLA PHY @ 00:01:08.640

BTS unit: 2:1
Channel No: 0 Name: PRACH
CFN: 217

Message Details:

Configuration Parameters:

Channel Offset:10240
Scrambling Code:16780416
Symbol Rate:60k
Channelization Code:128
Adjust Time:0
Slot Format:2
NumOfDpdch:1

#### CPHY Radio Link Setup CNF

PHY LLA @ 00:01:08.640

BTS unit: 2:1
Channel No: 0 Name: PRACH
CFN: 217

Message Details:

#### CPHY_RL_Setup_CNF

LLA RRC @ 00:01:08.650

Channel ID: AICH#1
Cell ID: 3

Message Details:

CPHY_RL_Setup_CNF:

cellId:3

routingInfo:

physicalChannelIdentity:7

#### CPHY_RL_Setup_REQ

RRC LLA @ 00:01:08.650

Channel ID: PRACH#1
Cell ID: 3

Message Details:

CPHY_RL_Setup_REQ:

cellId:3

routingInfo:

physicalChannelIdentity:8

ratType:fdd

setupMessage: (CphyRlSetupReq)

physicalChannelInfo:

pRACHInfo:

fdd_tdd:

fdd:

preambleSignature (AvailableSignatures):0000000011111111
spreadingFactorForDataPart (SF_PRACH):sfpr64
preambleScramblingCode (PreambleScramblingCodeWordNumber):0
puncturingLimit:pl1
accessSlot (AvailableSubChannelNumbers):111111111111

#### CPHY Transport Channel Configuration REQ

LLA PHY @ 00:01:08.660

BTS unit: 2:1
Channel No: 0 Name: PRACH
CFN: 219

Message Details:

Configuration Parameters:

DTX Position:Flexible
Second Interleave:On
Puncture Limit:100
CCTrCH Length:600
Number Of Transport Channels:1

Transport Channels:

Item Number 0:

Transport Channel Parameters:

Transport Channel:

Name:RACH
Identity:0

TTI (ms):20
EP Type:1/2 Rate Convolutional Coding
CRC Size:16
RM Attribute:150
First Interleave:On
Number Of Transport Formats:2

Transport Format Set:

Transport Format 0:

Number Of Transport Blocks:1
Transport Block Size In Bits:168

Transport Format 1:

Number Of Transport Blocks:1
Transport Block Size In Bits:360

RM Maximum Length:600

Transport Format Combination Set:

Number Of Transport Format Combinations:2

Transport Format Combinations 0:

Transport Format:0

Transport Format Combinations 1:

Transport Format:1

#### CPHY Transport Channel Configuration CNF

PHY LLA @ 00:01:08.670

BTS unit: 2:1
Channel No: 0 Name: PRACH
CFN: 220

Message Details:

#### CPHY_RL_Setup_CNF

LLA RRC @ 00:01:08.670

Channel ID: PRACH#1
Cell ID: 3

Message Details:

CPHY_RL_Setup_CNF:

cellId:3

routingInfo:

physicalChannelIdentity:8

#### CPHY_TrCH_Config_REQ

RRC LLA @ 00:01:08.670

Channel ID: PRACH#1
Cell ID: 3

Message Details:

CPHY_TrCH_Config_REQ:

cellId:3

routingInfo:

physicalChannelIdentity:8

ratType:fdd

trchConfigType:

nonDch:

configMessage: (CphyTrchConfigReq)

activationTime: (SS_ActivationTime)

activateNow:

ulconnectedTrCHList:

:

trchid (TransportChannelIdentity):15
ul_TransportChannelType (SS_UL_TransportChannelType):rach

transportChannelInfo: (CommonOrDedicatedTFS)

tti:

tti20: (CommonOrDedicatedTF_InfoList)

CommonOrDedicatedTF_Info:

tb_Size:168

numberOfTbSizeList:

NumberOfTransportBlocks:

one:

logicalChannelList:

configured:

CommonOrDedicatedTF_Info:

tb_Size:360

numberOfTbSizeList:

NumberOfTransportBlocks:

one:

logicalChannelList:

configured:

semistaticTF_Information:

channelCodingType:

convolutional (CodingRate):half

rateMatchingAttribute:150
crc_Size:crc16

ulTFCS: (TFCS)

normalTFCI_Signalling: (ExplicitTFCS_Configuration)

complete: (TFCS_ReconfAdd)

ctfcSize:

ctfc2Bit:

:

ctfc2:0

powerOffsetInformation: Omit

:

ctfc2:1

powerOffsetInformation: Omit

dlconnectedTrCHList: Omit

dlTFCS: (TFCS) Omit

#### CMAC Configuration REQ

LLA MAC @ 00:01:08.690

BTS unit: 2:1
Channel No: 0 Name: PRACH
CFN: 222

Message Details:

Configuration Parameters:

Number Of Transport Channels:1

Transport Channels:

Item Number 0:

Transport Channel Parameters:

Transport Channel:

Name:RACH
Identity:0

TTI (ms):20
EP Type:1/2 Rate Convolutional Coding
CRC Size:16
RM Attribute:150
First Interleave:On
Number Of Transport Formats:2

Transport Format Set:

Transport Format 0:

Number Of Transport Blocks:1
Transport Block Size In Bits:168

Transport Format 1:

Number Of Transport Blocks:1
Transport Block Size In Bits:360

Number Of Logical Channels:1

Logical Channels:

Item Number 0:

Logical Channel:

Name:CCCH
Identity:0

Priority:0
CT Length:0
CT Value:0
TCTF Length:2
TCTF Value:0
UE ID Type:Not used
UE ID:0

Active Flag:1

Transport Format Combination Set:

Number Of Transport Format Combinations:2

Transport Format Combinations 0:

Transport Format:0

Transport Format Combinations 1:

Transport Format:1

#### CMAC Configuration CNF

MAC LLA @ 00:01:08.690

BTS unit: 2:1
Channel No: 0 Name: PRACH
CFN: 222

Message Details:

#### CRLC TM Channel Establish REQ

LLA RLC @ 00:01:08.700

BTS unit: 2:1
Channel No: 0 Name: BCCH
CFN: 223

Message Details:

Configuration Parameters:

Number Of PU Sizes:1

PU sizes In Bits:

Item 0:246

#### CRLC TM Channel Establish CNF

RLC LLA @ 00:01:08.700

BTS unit: 2:1
Channel No: 0 Name: BCCH
CFN: 223

Message Details:

#### CPHY_TrCH_Config_CNF

LLA RRC @ 00:01:08.720

Channel ID: PRACH#1
Cell ID: 3

Message Details:

CPHY_TrCH_Config_CNF:

cellId:3

routingInfo:

physicalChannelIdentity:8

#### CMAC_Config_REQ

RRC LLA @ 00:01:08.720

Channel ID: PRACH#1
Cell ID: 3

Message Details:

CMAC_Config_REQ:

cellId:3

routingInfo:

physicalChannelIdentity:8

ratType:fdd

configMessage:

setup: (CmacConfigReq)

activationTime: (SS_ActivationTime)

activateNow:

uE_Info:

u_RNTI: Omit

c_RNTI: Omit

trCHInfo:

ulconnectedTrCHList:

:

trchid (TransportChannelIdentity):15

transportChannelInfo: (CommonOrDedicatedTFS)

tti:

tti20: (CommonOrDedicatedTF_InfoList)

CommonOrDedicatedTF_Info:

tb_Size:168

numberOfTbSizeList:

NumberOfTransportBlocks:

one:

logicalChannelList:

configured:

CommonOrDedicatedTF_Info:

tb_Size:360

numberOfTbSizeList:

NumberOfTransportBlocks:

one:

logicalChannelList:

configured:

semistaticTF_Information:

channelCodingType:

convolutional (CodingRate):half

rateMatchingAttribute:150
crc_Size:crc16

ulTFCS: (TFCS)

normalTFCI_Signalling: (ExplicitTFCS_Configuration)

complete: (TFCS_ReconfAdd)

ctfcSize:

ctfc2Bit:

:

ctfc2:0

powerOffsetInformation: Omit

:

ctfc2:1

powerOffsetInformation: Omit

dlconnectedTrCHList: Omit

dlTFCS: (TFCS) Omit

trCH_LogCHMapping: (TrCH_LogCHMappingList1)

ulconnectedTrCHList:

:

trchid (TransportChannelIdentity):15

trCH_LogCHMappingList:

TrCH_LogicalChannelMapping:

logicalChannel_Mapping:

ul_LogicalChannelMapping: (SS_UL_LogicalChannelMapping)

macHeaderManipulation (MAC_HeaderManipulation):normalMacHeader
ul_TransportChannelType (SS_UL_TransportChannelType):rach
logicalChannelIdentity:5
logicalChannelType:cCCH

rB_Identity:0
cn_DomainIdentity: Omit

dlconnectedTrCHList: Omit

#### CRLC TM Channel Establish REQ

LLA RLC @ 00:01:08.720

BTS unit: 2:1
Channel No: 0 Name: PCCH
CFN: 225

Message Details:

Configuration Parameters:

Number Of PU Sizes:1

PU sizes In Bits:

Item 0:240

#### CRLC TM Channel Establish CNF

RLC LLA @ 00:01:08.720

BTS unit: 2:1
Channel No: 0 Name: PCCH
CFN: 225

Message Details:

#### CMAC_Config_CNF

LLA RRC @ 00:01:08.730

Channel ID: PRACH#1
Cell ID: 3

Message Details:

CMAC_Config_CNF:

cellId:3

routingInfo:

physicalChannelIdentity:8

#### CRLC_Config_REQ

RRC LLA @ 00:01:08.730

Channel ID: RbBcch
Cell ID: 3

Message Details:

CRLC_Config_REQ:

cellId:3

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode) Omit

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):246

dl_RLCModeInfo: (UL_RLC_Mode)

ul_TM_RLC_Mode:

transmissionRLC_Discard: Omit

segmentationIndication:false

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity): Omit
dLlogicalChannelIdentity (LogicalChannelIdentity):1
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC UM Channel Establish REQ

LLA RLC @ 00:01:08.730

BTS unit: 2:1
Channel No: 1 Name: CCCH
CFN: 226

Message Details:

Configuration Parameters:

PU Size In Bits:152

#### CRLC UM Channel Establish CNF

RLC LLA @ 00:01:08.730

BTS unit: 2:1
Channel No: 1 Name: CCCH
CFN: 226

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:01:08.750

Channel ID: RbBcch
Cell ID: 3

Message Details:

CRLC_Config_CNF:

cellId:3

routingInfo:

rB_Identity:-1

#### CRLC_Config_REQ

RRC LLA @ 00:01:08.750

Channel ID: RbPcch
Cell ID: 3

Message Details:

CRLC_Config_REQ:

cellId:3

routingInfo:

rB_Identity:-2

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode) Omit

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):240

dl_RLCModeInfo: (UL_RLC_Mode)

ul_TM_RLC_Mode:

transmissionRLC_Discard: Omit

segmentationIndication:false

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity): Omit
dLlogicalChannelIdentity (LogicalChannelIdentity):1
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC TM Channel Establish REQ

LLA RLC @ 00:01:08.750

BTS unit: 2:1
Channel No: 0 Name: CCCH
CFN: 228

Message Details:

Configuration Parameters:

Number Of PU Sizes:1

PU sizes In Bits:

Item 0:166

#### CRLC TM Channel Establish CNF

RLC LLA @ 00:01:08.750

BTS unit: 2:1
Channel No: 0 Name: CCCH
CFN: 228

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:01:08.760

Channel ID: RbPcch
Cell ID: 3

Message Details:

CRLC_Config_CNF:

cellId:3

routingInfo:

rB_Identity:-2

#### CRLC_Config_REQ

RRC LLA @ 00:01:08.760

Channel ID: Rb0
Cell ID: 3

Message Details:

CRLC_Config_REQ:

cellId:3

routingInfo:

rB_Identity:0

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode) Omit

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):152

dl_RLCModeInfo: (UL_RLC_Mode)

ul_UM_RLC_Mode:

transmissionRLC_Discard:

timerBasedNoExplicit (NoExplicitDiscard):dt100

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity): Omit
dLlogicalChannelIdentity (LogicalChannelIdentity):5
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC_Config_CNF

LLA RRC @ 00:01:08.780

Channel ID: Rb0
Cell ID: 3

Message Details:

CRLC_Config_CNF:

cellId:3

routingInfo:

rB_Identity:0

#### CRLC_Config_REQ

RRC LLA @ 00:01:08.780

Channel ID: Rb0
Cell ID: 3

Message Details:

CRLC_Config_REQ:

cellId:3

routingInfo:

rB_Identity:0

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode)

dl_TM_RLC_Mode:

segmentationIndication:false

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):166

dl_RLCModeInfo: (UL_RLC_Mode)

ul_TM_RLC_Mode:

transmissionRLC_Discard: Omit

segmentationIndication:false

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity):5
dLlogicalChannelIdentity (LogicalChannelIdentity): Omit
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC_Config_CNF

LLA RRC @ 00:01:08.790

Channel ID: Rb0
Cell ID: 3

Message Details:

CRLC_Config_CNF:

cellId:3

routingInfo:

rB_Identity:0

#### MAC_DATA_REQ

RLC MAC @ 00:01:08.800

Category: Configuration
BTS unit: 2:1
Channel No: 0 Name: BCCH
CFN: 233

Message Details:

RLC PDU size (bits):224
RLC PDU (raw):

[0]00 0E 21 9D C4 00 05 88
[8]08 02 11 E0 14 3F FD F6
[16]E6 FF A5 5D 74 EF CF 4C
[24]42 60 00 04

#### o_SIB_PER_Encoding

RRC RRC @ 00:01:08.810

Category: TSO

Message Details:

Inputs:

SIB:

sIB1: (SysInfoType1)

cn_CommonGSM_MAP_NAS_SysInfo (NAS_SystemInformationGSM_MAP):

[0]00 01

cn_DomainSysInfoList:

CN_DomainSysInfo:

cn_DomainIdentity:ps_domain

cn_Type:

gsm_MAP (NAS_SystemInformationGSM_MAP):

[0]01 00

cn_DRX_CycleLengthCoeff (CN_DRX_CycleLengthCoefficient):7

CN_DomainSysInfo:

cn_DomainIdentity:cs_domain

cn_Type:

gsm_MAP (NAS_SystemInformationGSM_MAP):

[0]1E 01

cn_DRX_CycleLengthCoeff (CN_DRX_CycleLengthCoefficient):7

ue_ConnTimersAndConstants:

t_301:ms2000
n_301:2
t_302:ms4000
n_302:3
t_304:ms1000
n_304:3
t_305:m60
t_307:s50
t_308:ms320
t_309:8
t_310:ms320
n_310:5
t_311:ms500
t_312:5
n_312:s200
t_313:10
n_313:s20
t_314:s20
t_315:s30
n_315:s200
t_316:s50
t_317:s1800

ue_IdleTimersAndConstants:

t_300:ms4000
n_300:7
t_312:10
n_312:s200

v3a0NonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]11 00 01 00 00 00 00 00
[8]00 00 01 01 10 00 10 00
[16]00 00 10 00 00 00 00 10
[24]00 01 00 01 11 10 00 00
[32]00 01 01 00 00 11 11 11
[40]11 11 11 01 11 11 01 10
[48]11 10 01 10 11 11 11 11
[56]10 10 01 01 01 01 11 01
[64]01 11 01 00 11 10 11 11
[72]11 00 11 11 01 00 11

#### o_SIB_PER_Encoding

RRC RRC @ 00:01:08.810

Category: TSO

Message Details:

Inputs:

SIB:

sIB2: (SysInfoType2)

ura_IdentityList:

URA_Identity:0000000000000010

nonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]00 00 00 00 00 00 00 00
[8]00 10

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:01:08.810

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:3

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:10
bcch_ModificationTime: Omit

#### PHY_DATA_REQ

MAC PHY @ 00:01:08.810

BTS unit: 2:1
Channel No: 0 Name: BCH
CFN: 234

Message Details:

SIB repetition period:64
SIB position:20
SIB size:246
SIB (raw):

[0]00 0E 21 9D C4 00 05 88
[8]08 02 11 E0 14 3F FD F6
[16]E6 FF A5 5D 74 EF CF 4C
[24]42 60 00 04 00 00 00 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 0E 21 9D C4 00 05 88
[8]08 02 11 E0 14 3F FD F6
[16]E6 FF A5 5D 74 EF CF 4C
[24]42 60 00 04 00 00 00

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:01:08.830

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:3

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:01:08.830

Channel ID: RbBcch
Cell ID: 3

Message Details:

RLC_TR_DATA_REQ:

cellId:3

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

completeSIB_List:

CompleteSIBshort:

sib_Type:systemInformationBlockType1
sib_Data_variable:11000100000000000000010110001000000010000000001000010001111000000001010000111111111111011111011011100110111111111010010101011101011101001110111111001111010011

CompleteSIBshort:

sib_Type:systemInformationBlockType2
sib_Data_variable:00000000000000000010

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:01:08.830

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 20

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

completeSIB_List:

CompleteSIB_List.element:

sib_Type: systemInformationBlockType1_SIB_Type [enum=1]

sib_Data_variable: 11000100000000000000010110001000000010000000001000010001111000000001010000111111111111011111011011100110111111111010010101011101011101001110111111001111010011

CompleteSIB_List.element:

sib_Type: systemInformationBlockType2_SIB_Type [enum=2]

sib_Data_variable: 00000000000000000010

Layer 3 SDU:

[0]00 0E 21 9D C4 00 05 88
[8]08 02 11 E0 14 3F FD F6
[16]E6 FF A5 5D 74 EF CF 4C
[24]42 60 00 04

#### o_SIB_PER_Encoding

RRC RRC @ 00:01:08.830

Category: TSO

Message Details:

Inputs:

SIB:

sIB2: (SysInfoType2)

ura_IdentityList:

URA_Identity:0000000000000010

nonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]00 00 00 00 00 00 00 00
[8]00 10

#### o_SIB_PER_Encoding

RRC RRC @ 00:01:08.830

Category: TSO

Message Details:

Inputs:

SIB:

sIB1: (SysInfoType1)

cn_CommonGSM_MAP_NAS_SysInfo (NAS_SystemInformationGSM_MAP):

[0]00 01

cn_DomainSysInfoList:

CN_DomainSysInfo:

cn_DomainIdentity:ps_domain

cn_Type:

gsm_MAP (NAS_SystemInformationGSM_MAP):

[0]01 00

cn_DRX_CycleLengthCoeff (CN_DRX_CycleLengthCoefficient):7

CN_DomainSysInfo:

cn_DomainIdentity:cs_domain

cn_Type:

gsm_MAP (NAS_SystemInformationGSM_MAP):

[0]1E 01

cn_DRX_CycleLengthCoeff (CN_DRX_CycleLengthCoefficient):7

ue_ConnTimersAndConstants:

t_301:ms2000
n_301:2
t_302:ms4000
n_302:3
t_304:ms1000
n_304:3
t_305:m60
t_307:s50
t_308:ms320
t_309:8
t_310:ms320
n_310:5
t_311:ms500
t_312:5
n_312:s200
t_313:10
n_313:s20
t_314:s20
t_315:s30
n_315:s200
t_316:s50
t_317:s1800

ue_IdleTimersAndConstants:

t_300:ms4000
n_300:7
t_312:10
n_312:s200

v3a0NonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]11 00 01 00 00 00 00 00
[8]00 00 01 01 10 00 10 00
[16]00 00 10 00 00 00 00 10
[24]00 01 00 01 11 10 00 00
[32]00 01 01 00 00 11 11 11
[40]11 11 11 01 11 11 01 10
[48]11 10 01 10 11 11 11 11
[56]10 10 01 01 01 01 11 01
[64]01 11 01 00 11 10 11 11
[72]11 00 11 11 01 00 11

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:01:08.830

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:3

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:10
bcch_ModificationTime: Omit

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:01:08.840

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:3

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:01:08.840

Channel ID: RbBcch
Cell ID: 3

Message Details:

RLC_TR_DATA_REQ:

cellId:3

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

completeSIB_List:

CompleteSIBshort:

sib_Type:systemInformationBlockType1
sib_Data_variable:11000100000000000000010110001000000010000000001000010001111000000001010000111111111111011111011011100110111111111010010101011101011101001110111111001111010011

CompleteSIBshort:

sib_Type:systemInformationBlockType2
sib_Data_variable:00000000000000000010

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:01:08.840

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 20

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

completeSIB_List:

CompleteSIB_List.element:

sib_Type: systemInformationBlockType1_SIB_Type [enum=1]

sib_Data_variable: 11000100000000000000010110001000000010000000001000010001111000000001010000111111111111011111011011100110111111111010010101011101011101001110111111001111010011

CompleteSIB_List.element:

sib_Type: systemInformationBlockType2_SIB_Type [enum=2]

sib_Data_variable: 00000000000000000010

Layer 3 SDU:

[0]00 0E 21 9D C4 00 05 88
[8]08 02 11 E0 14 3F FD F6
[16]E6 FF A5 5D 74 EF CF 4C
[24]42 60 00 04

#### o_SIB_PER_Encoding

RRC RRC @ 00:01:08.860

Category: TSO

Message Details:

Inputs:

SIB:

sIB3: (SysInfoType3)

sib4indicator:true
cellIdentity:0000000000000000000000000011

cellSelectReselectInfo: (CellSelectReselectInfoSIB_3_4)

mappingInfo: Omit

cellSelectQualityMeasure:

cpich_RSCP:

modeSpecificInfo:

fdd:

s_Intrasearch (S_SearchQual):8
s_Intersearch (S_SearchQual):8
s_SearchHCS (S_SearchRXLEV): Omit

rat_List: (RAT_FDD_InfoList)

RAT_FDD_Info:

rat_Identifier:gsm
s_SearchRAT (S_SearchQual):-16
s_HCS_RAT (S_SearchRXLEV): Omit
s_Limit_SearchRAT (S_SearchQual):0

q_QualMin:-24
q_RxlevMin:-40

q_Hyst_l_S (Q_Hyst_S):2
t_Reselection_S:0

hcs_ServingCellInformation: Omit

maxAllowedUL_TX_Power:21

cellAccessRestriction:

cellBarred:

notBarred:

cellReservedForOperatorUse (ReservedIndicator):notReserved
cellReservationExtension (ReservedIndicator):notReserved

accessClassBarredList:

AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred

nonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]01 00 00 00 00 00 00 00
[8]00 00 00 00 00 00 11 00
[16]10 11 01 11 00 01 10 00
[24]00 00 00 00 00 01 00 00
[32]00 00 00 10 01 00 00 10
[40]00 00 01 00 01 11 11 11
[48]11 11 11 11 11 11 11 11

#### o_SIB_PER_Encoding

RRC RRC @ 00:01:08.860

Category: TSO

Message Details:

Inputs:

SIB:

sIB7: (SysInfoType7)

modeSpecificInfo:

fdd:

ul_Interference:-100

prach_Information_SIB5_List: (DynamicPersistenceLevelList)

DynamicPersistenceLevel:2

prach_Information_SIB6_List: (DynamicPersistenceLevelList)

DynamicPersistenceLevel:2

expirationTimeFactor: Omit

nonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]10 00 00 10 10 00 00 00
[8]10 00 00 01

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:01:08.860

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:3

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:7
bcch_ModificationTime: Omit

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:01:08.870

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:3

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:01:08.870

Channel ID: RbBcch
Cell ID: 3

Message Details:

RLC_TR_DATA_REQ:

cellId:3

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

completeSIB_List:

CompleteSIBshort:

sib_Type:systemInformationBlockType7
sib_Data_variable:100000101000000010000001

CompleteSIBshort:

sib_Type:systemInformationBlockType3
sib_Data_variable:0100000000000000000000000000110010110111000110000000000000010000000000100100001000000100011111111111111111111111

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:01:08.870

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 14

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

completeSIB_List:

CompleteSIB_List.element:

sib_Type: systemInformationBlockType7_SIB_Type [enum=7]

sib_Data_variable: 100000101000000010000001

CompleteSIB_List.element:

sib_Type: systemInformationBlockType3_SIB_Type [enum=3]

sib_Data_variable: 0100000000000000000000000000110010110111000110000000000000010000000000100100001000000100011111111111111111111111

Layer 3 SDU:

[0]00 0E 27 17 82 80 81 1B
[8]7A 00 00 00 65 B8 C0 00
[16]80 12 10 23 FF FF F8

#### o_SIB_PER_Encoding

RRC RRC @ 00:01:08.870

Category: TSO

Message Details:

Inputs:

SIB:

sIB4: (SysInfoType4)

cellIdentity:0000000000000000000000000011

cellSelectReselectInfo: (CellSelectReselectInfoSIB_3_4)

mappingInfo: Omit

cellSelectQualityMeasure:

cpich_RSCP:

modeSpecificInfo:

fdd:

s_Intrasearch (S_SearchQual):8
s_Intersearch (S_SearchQual):8
s_SearchHCS (S_SearchRXLEV): Omit

rat_List: (RAT_FDD_InfoList)

RAT_FDD_Info:

rat_Identifier:gsm
s_SearchRAT (S_SearchQual):-16
s_HCS_RAT (S_SearchRXLEV): Omit
s_Limit_SearchRAT (S_SearchQual):0

q_QualMin:-24
q_RxlevMin:-40

q_Hyst_l_S (Q_Hyst_S):0
t_Reselection_S:0

hcs_ServingCellInformation: Omit

maxAllowedUL_TX_Power:21

cellAccessRestriction:

cellBarred:

notBarred:

cellReservedForOperatorUse (ReservedIndicator):notReserved
cellReservationExtension (ReservedIndicator):notReserved

accessClassBarredList: Omit

nonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]00 00 00 00 00 00 00 00
[8]00 00 00 00 00 01 10 01
[16]01 10 11 10 00 11 00 00
[24]00 00 00 00 00 10 00 00
[32]00 00 01 00 10 00 00 00
[40]00 00 10 00 11 10 11 1

#### o_SIB_PER_Encoding

RRC RRC @ 00:01:08.870

Category: TSO

Message Details:

Inputs:

SIB:

sIB7: (SysInfoType7)

modeSpecificInfo:

fdd:

ul_Interference:-100

prach_Information_SIB5_List: (DynamicPersistenceLevelList)

DynamicPersistenceLevel:2

prach_Information_SIB6_List: (DynamicPersistenceLevelList)

DynamicPersistenceLevel:2

expirationTimeFactor: Omit

nonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]10 00 00 10 10 00 00 00
[8]10 00 00 01

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:01:08.870

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:3

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:31
bcch_ModificationTime: Omit

#### MAC_DATA_REQ

RLC MAC @ 00:01:08.880

Category: Configuration
BTS unit: 2:1
Channel No: 0 Name: BCCH
CFN: 241

Message Details:

RLC PDU size (bits):224
RLC PDU (raw):

[0]00 0E 21 9D C4 00 05 88
[8]08 02 11 E0 14 3F FD F6
[16]E6 FF A5 5D 74 EF CF 4C
[24]42 60 00 04

#### MAC_DATA_REQ

RLC MAC @ 00:01:08.880

Category: Configuration
BTS unit: 2:1
Channel No: 0 Name: BCCH
CFN: 241

Message Details:

RLC PDU size (bits):184
RLC PDU (raw):

[0]00 0E 27 17 82 80 81 1B
[8]7A 00 00 00 65 B8 C0 00
[16]80 12 10 23 FF FF F8

#### MAC_DATA_REQ

RLC MAC @ 00:01:08.880

Category: Configuration
BTS unit: 2:1
Channel No: 0 Name: BCCH
CFN: 241

Message Details:

RLC PDU size (bits):168
RLC PDU (raw):

[0]00 0E 27 17 82 80 81 22
[8]F0 00 00 00 CB 71 80 01
[16]00 24 00 47 70

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:01:08.890

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:3

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:01:08.890

Channel ID: RbBcch
Cell ID: 3

Message Details:

RLC_TR_DATA_REQ:

cellId:3

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

completeSIB_List:

CompleteSIBshort:

sib_Type:systemInformationBlockType7
sib_Data_variable:100000101000000010000001

CompleteSIBshort:

sib_Type:systemInformationBlockType4
sib_Data_variable:00000000000000000000000000011001011011100011000000000000001000000000010010000000000010001110111

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:01:08.890

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 62

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

completeSIB_List:

CompleteSIB_List.element:

sib_Type: systemInformationBlockType7_SIB_Type [enum=7]

sib_Data_variable: 100000101000000010000001

CompleteSIB_List.element:

sib_Type: systemInformationBlockType4_SIB_Type [enum=4]

sib_Data_variable: 00000000000000000000000000011001011011100011000000000000001000000000010010000000000010001110111

Layer 3 SDU:

[0]00 0E 27 17 82 80 81 22
[8]F0 00 00 00 CB 71 80 01
[16]00 24 00 47 70

#### PHY_DATA_REQ

MAC PHY @ 00:01:08.890

BTS unit: 2:1
Channel No: 0 Name: BCH
CFN: 242

Message Details:

SIB repetition period:64
SIB position:20
SIB size:246
SIB (raw):

[0]00 0E 21 9D C4 00 05 88
[8]08 02 11 E0 14 3F FD F6
[16]E6 FF A5 5D 74 EF CF 4C
[24]42 60 00 04 00 00 00 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 0E 21 9D C4 00 05 88
[8]08 02 11 E0 14 3F FD F6
[16]E6 FF A5 5D 74 EF CF 4C
[24]42 60 00 04 00 00 00

#### o_SIB_PER_Encoding

RRC RRC @ 00:01:08.900

Category: TSO

Message Details:

Inputs:

SIB:

sIB5: (SysInfoType5)

sib6indicator:true
pich_PowerOffset:-5

modeSpecificInfo:

fdd:

aich_PowerOffset:-5

primaryCCPCH_Info: Omit

prach_SystemInformationList:

PRACH_SystemInformation:

prach_RACH_Info:

modeSpecificInfo:

fdd:

availableSignatures:0000000011111111
availableSF (SF_PRACH):sfpr64
preambleScramblingCodeWordNumber:0
puncturingLimit:pl1
availableSubChannelNumbers:111111111111

transportChannelIdentity:15

rach_TransportFormatSet: (TransportFormatSet)

commonTransChTFS:

tti:

tti20: (CommonDynamicTF_InfoList)

CommonDynamicTF_Info:

rlc_Size:

fdd:

octetModeRLC_SizeInfoType2:

sizeType1:15

numberOfTbSizeList:

NumberOfTransportBlocks:

one:

logicalChannelList:

configured:

CommonDynamicTF_Info:

rlc_Size:

fdd:

octetModeRLC_SizeInfoType2:

sizeType2:3

numberOfTbSizeList:

NumberOfTransportBlocks:

one:

logicalChannelList:

configured:

semistaticTF_Information:

channelCodingType:

convolutional (CodingRate):half

rateMatchingAttribute:150
crc_Size:crc16

rach_TFCS: (TFCS)

normalTFCI_Signalling: (ExplicitTFCS_Configuration)

complete: (TFCS_ReconfAdd)

ctfcSize:

ctfc2Bit:

:

ctfc2:0

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m:0

:

ctfc2:1

powerOffsetInformation:

gainFactorInformation:

signalledGainFactors:

modeSpecificInfo:

fdd:

gainFactorBetaC (GainFactor):11

gainFactorBetaD (GainFactor):15
referenceTFC_ID:0

powerOffsetPp_m:0

prach_Partitioning:

fdd:

ASCSetting_FDD:

accessServiceClass_FDD: Omit

ASCSetting_FDD:

accessServiceClass_FDD:

availableSignatureStartIndex:0
availableSignatureEndIndex:7
assignedSubChannelNumber:1111

ASCSetting_FDD:

accessServiceClass_FDD: Omit

ASCSetting_FDD:

accessServiceClass_FDD:

availableSignatureStartIndex:0
availableSignatureEndIndex:7
assignedSubChannelNumber:1111

ASCSetting_FDD:

accessServiceClass_FDD: Omit

ASCSetting_FDD:

accessServiceClass_FDD:

availableSignatureStartIndex:0
availableSignatureEndIndex:7
assignedSubChannelNumber:1111

ASCSetting_FDD:

accessServiceClass_FDD: Omit

ASCSetting_FDD:

accessServiceClass_FDD:

availableSignatureStartIndex:0
availableSignatureEndIndex:7
assignedSubChannelNumber:1111

persistenceScalingFactorList:

PersistenceScalingFactor:psf0_9
PersistenceScalingFactor:psf0_9
PersistenceScalingFactor:psf0_9
PersistenceScalingFactor:psf0_9
PersistenceScalingFactor:psf0_9
PersistenceScalingFactor:psf0_9

ac_To_ASC_MappingTable:

AC_To_ASC_Mapping:6
AC_To_ASC_Mapping:5
AC_To_ASC_Mapping:4
AC_To_ASC_Mapping:3
AC_To_ASC_Mapping:2
AC_To_ASC_Mapping:1
AC_To_ASC_Mapping:0

modeSpecificInfo:

fdd:

primaryCPICH_TX_Power:31
constantValue:-10

prach_PowerOffset:

powerRampStep:3
preambleRetransMax:4

rach_TransmissionParameters:

mmax:2
nb01Min (NB01):3
nb01Max (NB01):10

aich_Info:

channelisationCode256:3
sttd_Indicator:false
aich_TransmissionTiming:e0

sCCPCH_SystemInformationList:

SCCPCH_SystemInformation:

secondaryCCPCH_Info:

modeSpecificInfo:

fdd:

dummy1 (PCPICH_UsageForChannelEst):mayBeUsed

dummy2: (SecondaryCPICH_Info) Omit

secondaryScramblingCode: Omit
sttd_Indicator:false

sf_AndCodeNumber: (SF256_AndCodeNumber)

sf64:1

pilotSymbolExistence:false
tfci_Existence:true
positionFixedOrFlexible:flexible
timingOffset:0

tfcs:

normalTFCI_Signalling: (ExplicitTFCS_Configuration)

complete: (TFCS_ReconfAdd)

ctfcSize:

ctfc4Bit:

:

ctfc4:0

powerOffsetInformation: Omit

:

ctfc4:1

powerOffsetInformation: Omit

:

ctfc4:2

powerOffsetInformation: Omit

:

ctfc4:3

powerOffsetInformation: Omit

:

ctfc4:4

powerOffsetInformation: Omit

:

ctfc4:5

powerOffsetInformation: Omit

:

ctfc4:6

powerOffsetInformation: Omit

:

ctfc4:8

powerOffsetInformation: Omit

fach_PCH_InformationList:

FACH_PCH_Information:

transportFormatSet:

commonTransChTFS:

tti:

tti10: (CommonDynamicTF_InfoList)

CommonDynamicTF_Info:

rlc_Size:

fdd:

octetModeRLC_SizeInfoType2:

sizeType1:24

numberOfTbSizeList:

NumberOfTransportBlocks:

zero:

NumberOfTransportBlocks:

one:

logicalChannelList:

allSizes:

semistaticTF_Information:

channelCodingType:

convolutional (CodingRate):half

rateMatchingAttribute:230
crc_Size:crc16

transportChannelIdentity:12
ctch_Indicator:false

FACH_PCH_Information:

transportFormatSet:

commonTransChTFS:

tti:

tti10: (CommonDynamicTF_InfoList)

CommonDynamicTF_Info:

rlc_Size:

fdd:

octetModeRLC_SizeInfoType2:

sizeType1:15

numberOfTbSizeList:

NumberOfTransportBlocks:

zero:

NumberOfTransportBlocks:

one:

NumberOfTransportBlocks:

small:2

logicalChannelList:

allSizes:

semistaticTF_Information:

channelCodingType:

convolutional (CodingRate):half

rateMatchingAttribute:220
crc_Size:crc16

transportChannelIdentity:13
ctch_Indicator:false

FACH_PCH_Information:

transportFormatSet:

commonTransChTFS:

tti:

tti10: (CommonDynamicTF_InfoList)

CommonDynamicTF_Info:

rlc_Size:

fdd:

octetModeRLC_SizeInfoType2:

sizeType2:3

numberOfTbSizeList:

NumberOfTransportBlocks:

zero:

NumberOfTransportBlocks:

one:

logicalChannelList:

allSizes:

semistaticTF_Information:

channelCodingType:

turbo:

rateMatchingAttribute:130
crc_Size:crc16

transportChannelIdentity:14
ctch_Indicator:false

pich_Info:

fdd:

channelisationCode256:2
pi_CountPerFrame:e18
sttd_Indicator:false

cbs_DRX_Level1Information: Omit

nonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]00 01 01 01 01 00 01 00
[8]00 11 11 10 00 00 00 00
[16]11 11 11 11 01 00 00 11
[24]11 11 11 11 11 11 11 01
[32]11 01 00 10 00 01 00 00
[40]11 11 00 00 00 10 10 01
[48]00 00 11 00 00 00 10 10
[56]10 10 01 01 01 01 10 00
[64]00 00 00 00 00 00 11 00
[72]11 00 01 01 10 11 01 01
[80]01 11 11 10 00 10 10 11
[88]10 10 00 00 11 11 11 10
[96]10 00 00 11 11 11 10 10
[104]00 00 11 11 11 10 10 00
[112]00 11 11 11 11 01 00 00
[120]00 00 00 00 00 00 00 11
[128]01 01 10 00 11 01 00 01
[136]00 00 11 11 11 01 00 11
[144]10 01 01 00 00 01 10 00
[152]01 00 00 11 00 10 10 00
[160]00 00 11 00 00 00 11 10
[168]00 00 01 00 00 00 01 01
[176]10 00 00 10 00 00 00 11
[184]10 00 00 00 00 10 00 10
[192]00 01 10 01 00 00 10 10
[200]01 10 01 00 00 10 10 00
[208]00 00 00 00 11 00 00 00
[216]01 00 01 00 01 01 11 00
[224]10 10 11 01 01 10 10 00
[232]00 00 00 00 01 11 10 00
[240]10 00 01 10 00 00 00 01
[248]01 10 11 01 10 11 01 10
[256]00 10 00 00 00 00 01 00
[264]00 11 00 00 10 00 10 01
[272]01 00 00 00 10 11 01 10
[280]10 00 00 00 01 00 00

#### PHY_DATA_REQ

MAC PHY @ 00:01:08.910

BTS unit: 2:1
Channel No: 0 Name: BCH
CFN: 244

Message Details:

SIB repetition period:64
SIB position:14
SIB size:246
SIB (raw):

[0]00 0E 27 17 82 80 81 1B
[8]7A 00 00 00 65 B8 C0 00
[16]80 12 10 23 FF FF F8 4C
[24]42 60 00 04 00 00 00 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 0E 27 17 82 80 81 1B
[8]7A 00 00 00 65 B8 C0 00
[16]80 12 10 23 FF FF F8 4C
[24]42 60 00 04 00 00 00

#### MAC_DATA_REQ

RLC MAC @ 00:01:08.920

Category: Configuration
BTS unit: 2:1
Channel No: 0 Name: BCCH
CFN: 245

Message Details:

RLC PDU size (bits):16
RLC PDU (raw):

[0]00 00

#### PHY_DATA_REQ

MAC PHY @ 00:01:08.930

BTS unit: 2:1
Channel No: 0 Name: BCH
CFN: 246

Message Details:

SIB repetition period:64
SIB position:62
SIB size:246
SIB (raw):

[0]00 0E 27 17 82 80 81 22
[8]F0 00 00 00 CB 71 80 01
[16]00 24 00 47 70 FF F8 4C
[24]42 60 00 04 00 00 00 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 0E 27 17 82 80 81 22
[8]F0 00 00 00 CB 71 80 01
[16]00 24 00 47 70 FF F8 4C
[24]42 60 00 04 00 00 00

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:01:08.940

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:3

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:22
bcch_ModificationTime: Omit

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:01:08.950

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:3

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:01:08.950

Channel ID: RbBcch
Cell ID: 3

Message Details:

RLC_TR_DATA_REQ:

cellId:3

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

noSegment:

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:01:08.950

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 44

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

noSegment: NULL

Layer 3 SDU:

[0]00 00

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:01:08.950

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:3

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:18
bcch_ModificationTime: Omit

#### PHY_DATA_REQ

MAC PHY @ 00:01:08.950

BTS unit: 2:1
Channel No: 0 Name: BCH
CFN: 248

Message Details:

SIB repetition period:64
SIB position:44
SIB size:246
SIB (raw):

[0]00 00 27 17 82 80 81 22
[8]F0 00 00 00 CB 71 80 01
[16]00 24 00 47 70 FF F8 4C
[24]42 60 00 04 00 00 00 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 00 27 17 82 80 81 22
[8]F0 00 00 00 CB 71 80 01
[16]00 24 00 47 70 FF F8 4C
[24]42 60 00 04 00 00 00

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:01:08.970

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:3

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:01:08.970

Channel ID: RbBcch
Cell ID: 3

Message Details:

RLC_TR_DATA_REQ:

cellId:3

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

firstSegment:

sib_Type:systemInformationBlockType5
seg_Count (SegCount):3
sib_Data_fixed:000101010100010000111110000000001111111101000011111111111111110111010010000100001111000000101001000011000000101010100101010110000000000000001100110001011011010101111110001010111010000011111110100000111111101000001111111010

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:01:08.970

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 36

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

firstSegment:

sib_Type: systemInformationBlockType5_SIB_Type [enum=5]

seg_Count: 3

sib_Data_fixed: 000101010100010000111110000000001111111101000011111111111111110111010010000100001111000000101001000011000000101010100101010110000000000000001100110001011011010101111110001010111010000011111110100000111111101000001111111010

Layer 3 SDU:

[0]00 02 52 15 44 3E 00 FF
[8]43 FF FD D2 10 F0 29 0C
[16]0A A5 58 00 0C C5 B5 7E
[24]2B A0 FE 83 FA 0F E8

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:01:08.970

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:3

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:19
bcch_ModificationTime: Omit

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:01:08.980

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:3

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:01:08.980

Channel ID: RbBcch
Cell ID: 3

Message Details:

RLC_TR_DATA_REQ:

cellId:3

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

subsequentSegment:

sib_Type:systemInformationBlockType5
segmentIndex:1
sib_Data_fixed:000011111111010000000000000000001101011000110100010000111111010011100101000001100001000011001010000000110000001110000001000000010110000010000000111000000000100010000110010000101001100100001010000000000011000000010001000101

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:01:08.980

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 38

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

subsequentSegment:

sib_Type: systemInformationBlockType5_SIB_Type [enum=5]

segmentIndex: 1

sib_Data_fixed: 000011111111010000000000000000001101011000110100010000111111010011100101000001100001000011001010000000110000001110000001000000010110000010000000111000000000100010000110010000101001100100001010000000000011000000010001000101

Layer 3 SDU:

[0]00 04 50 0F F4 00 00 D6
[8]34 43 F4 E5 06 10 CA 03
[16]03 81 01 60 80 E0 08 86
[24]42 99 0A 00 30 11 14

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:01:08.980

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:3

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:21
bcch_ModificationTime: Omit

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:01:09.000

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:3

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:01:09.000

Channel ID: RbBcch
Cell ID: 3

Message Details:

RLC_TR_DATA_REQ:

cellId:3

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

lastSegmentShort:

sib_Type:systemInformationBlockType5
segmentIndex:2
sib_Data_variable:1100101011010110100000000000011110001000011000000001011011011011011000100000000001000011000010001001010000001011011010000000010000

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:01:09.000

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 42

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

lastSegmentShort:

sib_Type: systemInformationBlockType5_SIB_Type [enum=5]

segmentIndex: 2

sib_Data_variable: 1100101011010110100000000000011110001000011000000001011011011011011000100000000001000011000010001001010000001011011010000000010000

Layer 3 SDU:

[0]00 06 51 81 CA D6 80 07
[8]88 60 16 DB 62 00 43 08
[16]94 0B 68 04 00

#### o_SIB_PER_Encoding

RRC RRC @ 00:01:09.000

Category: TSO

Message Details:

Inputs:

SIB:

sIB6: (SysInfoType6)

pich_PowerOffset:-5

modeSpecificInfo:

fdd:

aich_PowerOffset:-5
dummy (CSICH_PowerOffset): Omit

primaryCCPCH_Info: Omit

prach_SystemInformationList: Omit

sCCPCH_SystemInformationList: Omit

cbs_DRX_Level1Information: Omit

nonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]00 00 00 10 10 01 00 01

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:01:09.000

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:3

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:2
bcch_ModificationTime: Omit

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:01:09.010

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:3

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:01:09.010

Channel ID: RbBcch
Cell ID: 3

Message Details:

RLC_TR_DATA_REQ:

cellId:3

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

completeSIB_List:

CompleteSIBshort:

sib_Type:systemInformationBlockType6
sib_Data_variable:0000001010010001

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:01:09.010

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 4

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

completeSIB_List:

CompleteSIB_List.element:

sib_Type: systemInformationBlockType6_SIB_Type [enum=6]

sib_Data_variable: 0000001010010001

Layer 3 SDU:

[0]00 0E 06 0F 02 91

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:01:09.010

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:3

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:3
bcch_ModificationTime: Omit

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:01:09.030

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:3

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:01:09.030

Channel ID: RbBcch
Cell ID: 3

Message Details:

RLC_TR_DATA_REQ:

cellId:3

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

noSegment:

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:01:09.030

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 6

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

noSegment: NULL

Layer 3 SDU:

[0]00 00

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:01:09.030

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:3

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:5
bcch_ModificationTime: Omit

#### MAC_DATA_REQ

RLC MAC @ 00:01:09.030

Category: Configuration
BTS unit: 2:1
Channel No: 0 Name: BCCH
CFN: 0

Message Details:

RLC PDU size (bits):248
RLC PDU (raw):

[0]00 02 52 15 44 3E 00 FF
[8]43 FF FD D2 10 F0 29 0C
[16]0A A5 58 00 0C C5 B5 7E
[24]2B A0 FE 83 FA 0F E8

#### MAC_DATA_REQ

RLC MAC @ 00:01:09.030

Category: Configuration
BTS unit: 2:1
Channel No: 0 Name: BCCH
CFN: 0

Message Details:

RLC PDU size (bits):248
RLC PDU (raw):

[0]00 04 50 0F F4 00 00 D6
[8]34 43 F4 E5 06 10 CA 03
[16]03 81 01 60 80 E0 08 86
[24]42 99 0A 00 30 11 14

#### MAC_DATA_REQ

RLC MAC @ 00:01:09.030

Category: Configuration
BTS unit: 2:1
Channel No: 0 Name: BCCH
CFN: 0

Message Details:

RLC PDU size (bits):168
RLC PDU (raw):

[0]00 06 51 81 CA D6 80 07
[8]88 60 16 DB 62 00 43 08
[16]94 0B 68 04 00

#### MAC_DATA_REQ

RLC MAC @ 00:01:09.030

Category: Configuration
BTS unit: 2:1
Channel No: 0 Name: BCCH
CFN: 0

Message Details:

RLC PDU size (bits):48
RLC PDU (raw):

[0]00 0E 06 0F 02 91

#### MAC_DATA_REQ

RLC MAC @ 00:01:09.030

Category: Configuration
BTS unit: 2:1
Channel No: 0 Name: BCCH
CFN: 0

Message Details:

RLC PDU size (bits):16
RLC PDU (raw):

[0]00 00

#### MAC_DATA_REQ

RLC MAC @ 00:01:09.030

Category: Configuration
BTS unit: 2:1
Channel No: 0 Name: BCCH
CFN: 0

Message Details:

RLC PDU size (bits):16
RLC PDU (raw):

[0]00 00

#### PHY_DATA_REQ

MAC PHY @ 00:01:09.030

BTS unit: 2:1
Channel No: 0 Name: BCH
CFN: 0

Message Details:

SIB repetition period:64
SIB position:36
SIB size:246
SIB (raw):

[0]00 02 52 15 44 3E 00 FF
[8]43 FF FD D2 10 F0 29 0C
[16]0A A5 58 00 0C C5 B5 7E
[24]2B A0 FE 83 FA 0F E8 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 02 52 15 44 3E 00 FF
[8]43 FF FD D2 10 F0 29 0C
[16]0A A5 58 00 0C C5 B5 7E
[24]2B A0 FE 83 FA 0F E8

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:01:09.040

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:3

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:01:09.040

Channel ID: RbBcch
Cell ID: 3

Message Details:

RLC_TR_DATA_REQ:

cellId:3

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

noSegment:

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:01:09.040

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 10

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

noSegment: NULL

Layer 3 SDU:

[0]00 00

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:01:09.040

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:3

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:6
bcch_ModificationTime: Omit

#### PHY_DATA_REQ

MAC PHY @ 00:01:09.050

BTS unit: 2:1
Channel No: 0 Name: BCH
CFN: 2

Message Details:

SIB repetition period:64
SIB position:38
SIB size:246
SIB (raw):

[0]00 04 50 0F F4 00 00 D6
[8]34 43 F4 E5 06 10 CA 03
[16]03 81 01 60 80 E0 08 86
[24]42 99 0A 00 30 11 14 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 04 50 0F F4 00 00 D6
[8]34 43 F4 E5 06 10 CA 03
[16]03 81 01 60 80 E0 08 86
[24]42 99 0A 00 30 11 14

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:01:09.060

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:3

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:01:09.060

Channel ID: RbBcch
Cell ID: 3

Message Details:

RLC_TR_DATA_REQ:

cellId:3

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

noSegment:

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:01:09.060

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 12

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

noSegment: NULL

Layer 3 SDU:

[0]00 00

#### o_SIB_PER_Encoding

RRC RRC @ 00:01:09.060

Category: TSO

Message Details:

Inputs:

SIB:

sIB7: (SysInfoType7)

modeSpecificInfo:

fdd:

ul_Interference:-100

prach_Information_SIB5_List: (DynamicPersistenceLevelList)

DynamicPersistenceLevel:2

prach_Information_SIB6_List: (DynamicPersistenceLevelList)

DynamicPersistenceLevel:2

expirationTimeFactor: Omit

nonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]10 00 00 10 10 00 00 00
[8]10 00 00 01

#### o_SIB_PER_Encoding

RRC RRC @ 00:01:09.060

Category: TSO

Message Details:

Inputs:

SIB:

sIB12: (SysInfoType12)

fach_MeasurementOccasionInfo: Omit

measurementControlSysInfo:

use_of_HCS:

hcs_not_used:

cellSelectQualityMeasure:

cpich_RSCP:

intraFreqMeasurementSysInfo: (IntraFreqMeasurementSysInfo_RSCP)

intraFreqMeasurementID (MeasurementIdentity): Omit

intraFreqCellInfoSI_List: (IntraFreqCellInfoSI_List_RSCP)

removedIntraFreqCellList: Omit

newIntraFreqCellList: (NewIntraFreqCellSI_List_RSCP)

NewIntraFreqCellSI_RSCP:

intraFreqCellID:4

cellInfo: (CellInfoSI_RSCP)

cellIndividualOffset: Omit

referenceTimeDifferenceToCell: Omit

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode:300

primaryCPICH_TX_Power: Omit
readSFN_Indicator:true
tx_DiversityIndicator:false

cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP)

q_OffsetS_N:0
maxAllowedUL_TX_Power:21

modeSpecificInfo:

fdd:

q_QualMin:-16
q_RxlevMin:-58

NewIntraFreqCellSI_RSCP:

intraFreqCellID:5

cellInfo: (CellInfoSI_RSCP)

cellIndividualOffset: Omit

referenceTimeDifferenceToCell: Omit

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode:350

primaryCPICH_TX_Power: Omit
readSFN_Indicator:true
tx_DiversityIndicator:false

cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP)

q_OffsetS_N:0
maxAllowedUL_TX_Power:21

modeSpecificInfo:

fdd:

q_QualMin:-16
q_RxlevMin:-58

intraFreqMeasQuantity:

filterCoefficient: Omit

modeSpecificInfo:

fdd:

intraFreqMeasQuantity_FDD:cpich_RSCP

intraFreqReportingQuantityForRACH: Omit

maxReportedCellsOnRACH: Omit

reportingInfoForCellDCH:

intraFreqReportingQuantity:

activeSetReportingQuantities: (CellReportingQuantities)

dummy (SFN_SFN_OTD_Type):noReport
cellIdentity_reportingIndicator:true
cellSynchronisationInfoReportingIndicator:false

modeSpecificInfo:

fdd:

cpich_Ec_N0_reportingIndicator:false
cpich_RSCP_reportingIndicator:true
pathloss_reportingIndicator:false

monitoredSetReportingQuantities: (CellReportingQuantities)

dummy (SFN_SFN_OTD_Type):noReport
cellIdentity_reportingIndicator:true
cellSynchronisationInfoReportingIndicator:true

modeSpecificInfo:

fdd:

cpich_Ec_N0_reportingIndicator:false
cpich_RSCP_reportingIndicator:true
pathloss_reportingIndicator:false

detectedSetReportingQuantities: (CellReportingQuantities) Omit

measurementReportingMode:

measurementReportTransferMode (TransferMode):acknowledgedModeRLC
periodicalOrEventTrigger:eventTrigger

reportCriteria: (CellDCH_ReportCriteria)

intraFreqReportingCriteria:

eventCriteriaList: (IntraFreqEventCriteriaList)

IntraFreqEventCriteria:

event: (IntraFreqEvent)

e1a: (Event1a)

triggeringCondition (TriggeringCondition2):monitoredSetCellsOnly
reportingRange:5

forbiddenAffectCellList: Omit

w:1
reportDeactivationThreshold:t2
reportingAmount:ra4
reportingInterval:noPeriodicalreporting

hysteresis:0
timeToTrigger:ttt640

reportingCellStatus:

withinActiveAndOrMonitoredUsedFreq (MaxNumberOfReportingCellsType1):e3

IntraFreqEventCriteria:

event: (IntraFreqEvent)

e1b: (Event1b)

triggeringCondition (TriggeringCondition1):activeSetCellsOnly
reportingRange:5

forbiddenAffectCellList: Omit

w:1

hysteresis:0
timeToTrigger:ttt640

reportingCellStatus:

withinActiveAndOrMonitoredUsedFreq (MaxNumberOfReportingCellsType1):e3

IntraFreqEventCriteria:

event: (IntraFreqEvent)

e1c: (Event1c)

replacementActivationThreshold:t3
reportingAmount:ra4
reportingInterval:ri4

hysteresis:0
timeToTrigger:ttt640

reportingCellStatus:

withinActiveAndOrMonitoredUsedFreq (MaxNumberOfReportingCellsType1):e3

interFreqMeasurementSysInfo: (InterFreqMeasurementSysInfo_RSCP)

interFreqCellInfoSI_List: (InterFreqCellInfoSI_List_RSCP)

removedInterFreqCellList: Omit

newInterFreqCellList: (NewInterFreqCellSI_List_RSCP)

NewInterFreqCellSI_RSCP:

interFreqCellID:0

frequencyInfo:

modeSpecificInfo:

fdd: (FrequencyInfoFDD)

uarfcn_UL (UARFCN):9613
uarfcn_DL (UARFCN):10563

cellInfo: (CellInfoSI_RSCP)

cellIndividualOffset: Omit

referenceTimeDifferenceToCell: Omit

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode:100

primaryCPICH_TX_Power: Omit
readSFN_Indicator:true
tx_DiversityIndicator:false

cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP)

q_OffsetS_N:0
maxAllowedUL_TX_Power:21

modeSpecificInfo:

fdd:

q_QualMin:-16
q_RxlevMin:-58

NewInterFreqCellSI_RSCP:

interFreqCellID:1

frequencyInfo: Omit

cellInfo: (CellInfoSI_RSCP)

cellIndividualOffset: Omit

referenceTimeDifferenceToCell: Omit

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode:150

primaryCPICH_TX_Power: Omit
readSFN_Indicator:true
tx_DiversityIndicator:false

cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP)

q_OffsetS_N:0
maxAllowedUL_TX_Power:21

modeSpecificInfo:

fdd:

q_QualMin:-16
q_RxlevMin:-58

NewInterFreqCellSI_RSCP:

interFreqCellID:2

frequencyInfo: Omit

cellInfo: (CellInfoSI_RSCP)

cellIndividualOffset: Omit

referenceTimeDifferenceToCell: Omit

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode:200

primaryCPICH_TX_Power: Omit
readSFN_Indicator:true
tx_DiversityIndicator:false

cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP)

q_OffsetS_N:0
maxAllowedUL_TX_Power:21

modeSpecificInfo:

fdd:

q_QualMin:-16
q_RxlevMin:-58

NewInterFreqCellSI_RSCP:

interFreqCellID:4

frequencyInfo:

modeSpecificInfo:

fdd: (FrequencyInfoFDD)

uarfcn_UL (UARFCN):9713
uarfcn_DL (UARFCN):10663

cellInfo: (CellInfoSI_RSCP)

cellIndividualOffset: Omit

referenceTimeDifferenceToCell: Omit

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode:150

primaryCPICH_TX_Power: Omit
readSFN_Indicator:true
tx_DiversityIndicator:false

cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP)

q_OffsetS_N:0
maxAllowedUL_TX_Power:21

modeSpecificInfo:

fdd:

q_QualMin:-16
q_RxlevMin:-58

NewInterFreqCellSI_RSCP:

interFreqCellID:7

frequencyInfo: Omit

cellInfo: (CellInfoSI_RSCP)

cellIndividualOffset: Omit

referenceTimeDifferenceToCell: Omit

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode:450

primaryCPICH_TX_Power: Omit
readSFN_Indicator:true
tx_DiversityIndicator:false

cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP)

q_OffsetS_N:0
maxAllowedUL_TX_Power:21

modeSpecificInfo:

fdd:

q_QualMin:-16
q_RxlevMin:-58

interRATMeasurementSysInfo: (InterRATMeasurementSysInfo_B) Omit

trafficVolumeMeasSysInfo: Omit

dummy: (UE_InternalMeasurementSysInfo) Omit

nonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]00 00 00 01 10 11 00 10
[8]00 00 11 00 10 00 01 01
[16]01 00 10 11 00 10 01 10
[24]00 11 10 01 10 10 00 00
[32]00 00 10 01 01 00 10 10
[40]10 10 11 11 01 00 11 00
[48]01 11 00 11 01 00 00 00
[56]00 00 00 10 00 10 00 10
[64]00 11 00 10 01 01 01 01
[72]00 00 00 01 00 10 10 00
[80]01 01 00 10 00 00 00 01
[88]10 00 01 00 10 10 00 10
[96]00 00 10 10 00 01 00 00
[104]11 00 00 10 01 01 00 10
[112]01 10 10 10 10 00 01 10
[120]00 01 00 10 10 10 01 00
[128]11 00 00 00 11 00 10 11
[136]00 01 10 11 01 00 10 10
[144]00 01 10 01 01 00 01 10
[152]01 00 10 01 10 00 11 10
[160]01 10 10 00 00 00 00 10
[168]00 00 10 01 01 00 10 01
[176]01 10 10 01 10 00 11 10
[184]01 10 10 00 00 00 00 10
[192]00 01 00 01 01 00 11 00
[200]10 00 10 01 10 00 11 10
[208]01 10 10 00 00 00 00 11
[216]00 10 00 11 00 10 11 11
[224]10 00 11 01 00 11 01 00
[232]11 10 01 01 00 10 01 01
[240]10 10 01 10 00 11 10 01
[248]10 10 00 00 00 00 10 00
[256]11 10 01 01 01 11 00 00
[264]10 10 01 10 00 11 10 01
[272]10 10 00 00 00 00

#### PHY_DATA_REQ

MAC PHY @ 00:01:09.070

BTS unit: 2:1
Channel No: 0 Name: BCH
CFN: 4

Message Details:

SIB repetition period:64
SIB position:42
SIB size:246
SIB (raw):

[0]00 06 51 81 CA D6 80 07
[8]88 60 16 DB 62 00 43 08
[16]94 0B 68 04 00 E0 08 86
[24]42 99 0A 00 30 11 14 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 06 51 81 CA D6 80 07
[8]88 60 16 DB 62 00 43 08
[16]94 0B 68 04 00 E0 08 86
[24]42 99 0A 00 30 11 14

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:01:09.080

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:3

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:15
bcch_ModificationTime: Omit

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:01:09.090

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:3

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:01:09.090

Channel ID: RbBcch
Cell ID: 3

Message Details:

RLC_TR_DATA_REQ:

cellId:3

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

completeSIB_List:

CompleteSIBshort:

sib_Type:systemInformationBlockType7
sib_Data_variable:100000101000000010000001

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:01:09.090

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 30

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

completeSIB_List:

CompleteSIB_List.element:

sib_Type: systemInformationBlockType7_SIB_Type [enum=7]

sib_Data_variable: 100000101000000010000001

Layer 3 SDU:

[0]00 0E 07 17 82 80 81

#### o_SIB_PER_Encoding

RRC RRC @ 00:01:09.090

Category: TSO

Message Details:

Inputs:

SIB:

sIB3: (SysInfoType3)

sib4indicator:true
cellIdentity:0000000000000000000000000011

cellSelectReselectInfo: (CellSelectReselectInfoSIB_3_4)

mappingInfo: Omit

cellSelectQualityMeasure:

cpich_RSCP:

modeSpecificInfo:

fdd:

s_Intrasearch (S_SearchQual):8
s_Intersearch (S_SearchQual):8
s_SearchHCS (S_SearchRXLEV): Omit

rat_List: (RAT_FDD_InfoList)

RAT_FDD_Info:

rat_Identifier:gsm
s_SearchRAT (S_SearchQual):-16
s_HCS_RAT (S_SearchRXLEV): Omit
s_Limit_SearchRAT (S_SearchQual):0

q_QualMin:-24
q_RxlevMin:-40

q_Hyst_l_S (Q_Hyst_S):2
t_Reselection_S:0

hcs_ServingCellInformation: Omit

maxAllowedUL_TX_Power:21

cellAccessRestriction:

cellBarred:

notBarred:

cellReservedForOperatorUse (ReservedIndicator):notReserved
cellReservationExtension (ReservedIndicator):notReserved

accessClassBarredList:

AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred

nonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]01 00 00 00 00 00 00 00
[8]00 00 00 00 00 00 11 00
[16]10 11 01 11 00 01 10 00
[24]00 00 00 00 00 01 00 00
[32]00 00 00 10 01 00 00 10
[40]00 00 01 00 01 11 11 11
[48]11 11 11 11 11 11 11 11

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:01:09.090

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:3

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:7
bcch_ModificationTime: Omit

#### PHY_DATA_REQ

MAC PHY @ 00:01:09.090

BTS unit: 2:1
Channel No: 0 Name: BCH
CFN: 6

Message Details:

SIB repetition period:64
SIB position:4
SIB size:246
SIB (raw):

[0]00 0E 06 0F 02 91 80 07
[8]88 60 16 DB 62 00 43 08
[16]94 0B 68 04 00 E0 08 86
[24]42 99 0A 00 30 11 14 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 0E 06 0F 02 91 80 07
[8]88 60 16 DB 62 00 43 08
[16]94 0B 68 04 00 E0 08 86
[24]42 99 0A 00 30 11 14

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:01:09.110

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:3

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:01:09.110

Channel ID: RbBcch
Cell ID: 3

Message Details:

RLC_TR_DATA_REQ:

cellId:3

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

completeSIB_List:

CompleteSIBshort:

sib_Type:systemInformationBlockType7
sib_Data_variable:100000101000000010000001

CompleteSIBshort:

sib_Type:systemInformationBlockType3
sib_Data_variable:0100000000000000000000000000110010110111000110000000000000010000000000100100001000000100011111111111111111111111

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:01:09.110

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 14

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

completeSIB_List:

CompleteSIB_List.element:

sib_Type: systemInformationBlockType7_SIB_Type [enum=7]

sib_Data_variable: 100000101000000010000001

CompleteSIB_List.element:

sib_Type: systemInformationBlockType3_SIB_Type [enum=3]

sib_Data_variable: 0100000000000000000000000000110010110111000110000000000000010000000000100100001000000100011111111111111111111111

Layer 3 SDU:

[0]00 0E 27 17 82 80 81 1B
[8]7A 00 00 00 65 B8 C0 00
[16]80 12 10 23 FF FF F8

#### PHY_DATA_REQ

MAC PHY @ 00:01:09.110

BTS unit: 2:1
Channel No: 0 Name: BCH
CFN: 8

Message Details:

SIB repetition period:64
SIB position:6
SIB size:246
SIB (raw):

[0]00 00 06 0F 02 91 80 07
[8]88 60 16 DB 62 00 43 08
[16]94 0B 68 04 00 E0 08 86
[24]42 99 0A 00 30 11 14 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 00 06 0F 02 91 80 07
[8]88 60 16 DB 62 00 43 08
[16]94 0B 68 04 00 E0 08 86
[24]42 99 0A 00 30 11 14

#### o_SIB_PER_Encoding

RRC RRC @ 00:01:09.120

Category: TSO

Message Details:

Inputs:

SIB:

sIB18: (SysInfoType18)

idleModePLMNIdentities: (PLMNIdentitiesOfNeighbourCells)

plmnsOfIntraFreqCellsList: Omit

plmnsOfInterFreqCellsList:

:

plmn_Identity:

mcc:

Digit:0
Digit:0
Digit:1

mnc:

Digit:0
Digit:1

:

plmn_Identity:

mcc:

Digit:0
Digit:0
Digit:1

mnc:

Digit:0
Digit:1

:

plmn_Identity:

mcc:

Digit:0
Digit:0
Digit:1

mnc:

Digit:0
Digit:1

:

plmn_Identity:

mcc:

Digit:0
Digit:0
Digit:4

mnc:

Digit:2
Digit:1

plmnsOfInterRATCellsList: Omit

connectedModePLMNIdentities: (PLMNIdentitiesOfNeighbourCells) Omit

nonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]10 00 10 00 01 11 00 00
[8]00 00 00 01 00 00 00 00
[16]11 00 00 00 00 00 01 00
[24]00 00 00 11 00 00 00 00
[32]00 01 00 00 00 00 11 00
[40]00 00 00 01 00 00 01 00
[48]00 1

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:01:09.120

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:3

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:23
bcch_ModificationTime: Omit

#### MAC_DATA_REQ

RLC MAC @ 00:01:09.120

Category: Configuration
BTS unit: 2:1
Channel No: 0 Name: BCCH
CFN: 9

Message Details:

RLC PDU size (bits):16
RLC PDU (raw):

[0]00 00

#### MAC_DATA_REQ

RLC MAC @ 00:01:09.120

Category: Configuration
BTS unit: 2:1
Channel No: 0 Name: BCCH
CFN: 9

Message Details:

RLC PDU size (bits):56
RLC PDU (raw):

[0]00 0E 07 17 82 80 81

#### MAC_DATA_REQ

RLC MAC @ 00:01:09.120

Category: Configuration
BTS unit: 2:1
Channel No: 0 Name: BCCH
CFN: 9

Message Details:

RLC PDU size (bits):184
RLC PDU (raw):

[0]00 0E 27 17 82 80 81 1B
[8]7A 00 00 00 65 B8 C0 00
[16]80 12 10 23 FF FF F8

#### MAC_DATA_REQ

RLC MAC @ 00:01:09.120

Category: Configuration
BTS unit: 2:1
Channel No: 0 Name: BCCH
CFN: 9

Message Details:

RLC PDU size (bits):168
RLC PDU (raw):

[0]00 0E 27 17 82 80 81 D3
[8]14 43 80 08 06 00 20 18
[16]00 80 60 08 21

#### MAC_DATA_REQ

RLC MAC @ 00:01:09.130

Category: Configuration
BTS unit: 2:1
Channel No: 0 Name: BCCH
CFN: 10

Message Details:

RLC PDU size (bits):168
RLC PDU (raw):

[0]00 0E 27 17 82 80 81 22
[8]F0 00 00 00 CB 71 80 01
[16]00 24 00 47 70

#### PHY_DATA_REQ

MAC PHY @ 00:01:09.130

BTS unit: 2:1
Channel No: 0 Name: BCH
CFN: 10

Message Details:

SIB repetition period:64
SIB position:10
SIB size:246
SIB (raw):

[0]00 00 06 0F 02 91 80 07
[8]88 60 16 DB 62 00 43 08
[16]94 0B 68 04 00 E0 08 86
[24]42 99 0A 00 30 11 14 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 00 06 0F 02 91 80 07
[8]88 60 16 DB 62 00 43 08
[16]94 0B 68 04 00 E0 08 86
[24]42 99 0A 00 30 11 14

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:01:09.140

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:3

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:01:09.140

Channel ID: RbBcch
Cell ID: 3

Message Details:

RLC_TR_DATA_REQ:

cellId:3

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

completeSIB_List:

CompleteSIBshort:

sib_Type:systemInformationBlockType7
sib_Data_variable:100000101000000010000001

CompleteSIBshort:

sib_Type:systemInformationBlockType18
sib_Data_variable:100010000111000000000001000000001100000000000100000000110000000000010000000011000000000100000100001

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:01:09.140

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 46

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

completeSIB_List:

CompleteSIB_List.element:

sib_Type: systemInformationBlockType7_SIB_Type [enum=7]

sib_Data_variable: 100000101000000010000001

CompleteSIB_List.element:

sib_Type: systemInformationBlockType18_SIB_Type [enum=26]

sib_Data_variable: 100010000111000000000001000000001100000000000100000000110000000000010000000011000000000100000100001

Layer 3 SDU:

[0]00 0E 27 17 82 80 81 D3
[8]14 43 80 08 06 00 20 18
[16]00 80 60 08 21

#### o_SIB_PER_Encoding

RRC RRC @ 00:01:09.140

Category: TSO

Message Details:

Inputs:

SIB:

sIB4: (SysInfoType4)

cellIdentity:0000000000000000000000000011

cellSelectReselectInfo: (CellSelectReselectInfoSIB_3_4)

mappingInfo: Omit

cellSelectQualityMeasure:

cpich_RSCP:

modeSpecificInfo:

fdd:

s_Intrasearch (S_SearchQual):8
s_Intersearch (S_SearchQual):8
s_SearchHCS (S_SearchRXLEV): Omit

rat_List: (RAT_FDD_InfoList)

RAT_FDD_Info:

rat_Identifier:gsm
s_SearchRAT (S_SearchQual):-16
s_HCS_RAT (S_SearchRXLEV): Omit
s_Limit_SearchRAT (S_SearchQual):0

q_QualMin:-24
q_RxlevMin:-40

q_Hyst_l_S (Q_Hyst_S):0
t_Reselection_S:0

hcs_ServingCellInformation: Omit

maxAllowedUL_TX_Power:21

cellAccessRestriction:

cellBarred:

notBarred:

cellReservedForOperatorUse (ReservedIndicator):notReserved
cellReservationExtension (ReservedIndicator):notReserved

accessClassBarredList: Omit

nonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]00 00 00 00 00 00 00 00
[8]00 00 00 00 00 01 10 01
[16]01 10 11 10 00 11 00 00
[24]00 00 00 00 00 10 00 00
[32]00 00 01 00 10 00 00 00
[40]00 00 10 00 11 10 11 1

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:01:09.140

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:3

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:31
bcch_ModificationTime: Omit

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:01:09.150

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:3

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:01:09.150

Channel ID: RbBcch
Cell ID: 3

Message Details:

RLC_TR_DATA_REQ:

cellId:3

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

completeSIB_List:

CompleteSIBshort:

sib_Type:systemInformationBlockType7
sib_Data_variable:100000101000000010000001

CompleteSIBshort:

sib_Type:systemInformationBlockType4
sib_Data_variable:00000000000000000000000000011001011011100011000000000000001000000000010010000000000010001110111

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:01:09.150

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 62

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

completeSIB_List:

CompleteSIB_List.element:

sib_Type: systemInformationBlockType7_SIB_Type [enum=7]

sib_Data_variable: 100000101000000010000001

CompleteSIB_List.element:

sib_Type: systemInformationBlockType4_SIB_Type [enum=4]

sib_Data_variable: 00000000000000000000000000011001011011100011000000000000001000000000010010000000000010001110111

Layer 3 SDU:

[0]00 0E 27 17 82 80 81 22
[8]F0 00 00 00 CB 71 80 01
[16]00 24 00 47 70

#### PHY_DATA_REQ

MAC PHY @ 00:01:09.150

BTS unit: 2:1
Channel No: 0 Name: BCH
CFN: 12

Message Details:

SIB repetition period:64
SIB position:12
SIB size:246
SIB (raw):

[0]00 00 06 0F 02 91 80 07
[8]88 60 16 DB 62 00 43 08
[16]94 0B 68 04 00 E0 08 86
[24]42 99 0A 00 30 11 14 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 00 06 0F 02 91 80 07
[8]88 60 16 DB 62 00 43 08
[16]94 0B 68 04 00 E0 08 86
[24]42 99 0A 00 30 11 14

#### PHY_DATA_REQ

MAC PHY @ 00:01:09.170

BTS unit: 2:1
Channel No: 0 Name: BCH
CFN: 14

Message Details:

SIB repetition period:64
SIB position:30
SIB size:246
SIB (raw):

[0]00 0E 07 17 82 80 81 07
[8]88 60 16 DB 62 00 43 08
[16]94 0B 68 04 00 E0 08 86
[24]42 99 0A 00 30 11 14 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 0E 07 17 82 80 81 07
[8]88 60 16 DB 62 00 43 08
[16]94 0B 68 04 00 E0 08 86
[24]42 99 0A 00 30 11 14

#### o_SIB_PER_Encoding

RRC RRC @ 00:01:09.190

Category: TSO

Message Details:

Inputs:

SIB:

sIB11: (SysInfoType11)

sib12indicator:true

fach_MeasurementOccasionInfo: Omit

measurementControlSysInfo:

use_of_HCS:

hcs_not_used:

cellSelectQualityMeasure:

cpich_RSCP:

intraFreqMeasurementSysInfo: (IntraFreqMeasurementSysInfo_RSCP)

intraFreqMeasurementID (MeasurementIdentity): Omit

intraFreqCellInfoSI_List: (IntraFreqCellInfoSI_List_RSCP)

removedIntraFreqCellList: Omit

newIntraFreqCellList: (NewIntraFreqCellSI_List_RSCP)

NewIntraFreqCellSI_RSCP:

intraFreqCellID:3

cellInfo: (CellInfoSI_RSCP)

cellIndividualOffset: Omit

referenceTimeDifferenceToCell: Omit

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode:200

primaryCPICH_TX_Power: Omit
readSFN_Indicator:false
tx_DiversityIndicator:false

cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP) Omit

NewIntraFreqCellSI_RSCP:

intraFreqCellID:4

cellInfo: (CellInfoSI_RSCP)

cellIndividualOffset: Omit

referenceTimeDifferenceToCell: Omit

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode:300

primaryCPICH_TX_Power: Omit
readSFN_Indicator:true
tx_DiversityIndicator:false

cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP)

q_OffsetS_N:0
maxAllowedUL_TX_Power:21

modeSpecificInfo:

fdd:

q_QualMin:-16
q_RxlevMin:-58

NewIntraFreqCellSI_RSCP:

intraFreqCellID:5

cellInfo: (CellInfoSI_RSCP)

cellIndividualOffset: Omit

referenceTimeDifferenceToCell: Omit

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode:350

primaryCPICH_TX_Power: Omit
readSFN_Indicator:true
tx_DiversityIndicator:false

cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP)

q_OffsetS_N:0
maxAllowedUL_TX_Power:21

modeSpecificInfo:

fdd:

q_QualMin:-16
q_RxlevMin:-58

intraFreqMeasQuantity:

filterCoefficient: Omit

modeSpecificInfo:

fdd:

intraFreqMeasQuantity_FDD:cpich_RSCP

intraFreqReportingQuantityForRACH: Omit

maxReportedCellsOnRACH: Omit

reportingInfoForCellDCH:

intraFreqReportingQuantity:

activeSetReportingQuantities: (CellReportingQuantities)

dummy (SFN_SFN_OTD_Type):noReport
cellIdentity_reportingIndicator:true
cellSynchronisationInfoReportingIndicator:false

modeSpecificInfo:

fdd:

cpich_Ec_N0_reportingIndicator:false
cpich_RSCP_reportingIndicator:true
pathloss_reportingIndicator:false

monitoredSetReportingQuantities: (CellReportingQuantities)

dummy (SFN_SFN_OTD_Type):noReport
cellIdentity_reportingIndicator:true
cellSynchronisationInfoReportingIndicator:true

modeSpecificInfo:

fdd:

cpich_Ec_N0_reportingIndicator:false
cpich_RSCP_reportingIndicator:true
pathloss_reportingIndicator:false

detectedSetReportingQuantities: (CellReportingQuantities) Omit

measurementReportingMode:

measurementReportTransferMode (TransferMode):acknowledgedModeRLC
periodicalOrEventTrigger:eventTrigger

reportCriteria: (CellDCH_ReportCriteria)

intraFreqReportingCriteria:

eventCriteriaList: (IntraFreqEventCriteriaList)

IntraFreqEventCriteria:

event: (IntraFreqEvent)

e1a: (Event1a)

triggeringCondition (TriggeringCondition2):monitoredSetCellsOnly
reportingRange:5

forbiddenAffectCellList: Omit

w:1
reportDeactivationThreshold:t2
reportingAmount:ra4
reportingInterval:ri4

hysteresis:0
timeToTrigger:ttt640

reportingCellStatus:

withinActiveAndOrMonitoredUsedFreq (MaxNumberOfReportingCellsType1):e3

IntraFreqEventCriteria:

event: (IntraFreqEvent)

e1b: (Event1b)

triggeringCondition (TriggeringCondition1):activeSetCellsOnly
reportingRange:5

forbiddenAffectCellList: Omit

w:1

hysteresis:0
timeToTrigger:ttt640

reportingCellStatus:

withinActiveAndOrMonitoredUsedFreq (MaxNumberOfReportingCellsType1):e3

IntraFreqEventCriteria:

event: (IntraFreqEvent)

e1c: (Event1c)

replacementActivationThreshold:t3
reportingAmount:ra4
reportingInterval:ri4

hysteresis:0
timeToTrigger:ttt640

reportingCellStatus:

withinActiveAndOrMonitoredUsedFreq (MaxNumberOfReportingCellsType1):e3

interFreqMeasurementSysInfo: (InterFreqMeasurementSysInfo_RSCP)

interFreqCellInfoSI_List: (InterFreqCellInfoSI_List_RSCP)

removedInterFreqCellList: Omit

newInterFreqCellList: (NewInterFreqCellSI_List_RSCP)

NewInterFreqCellSI_RSCP:

interFreqCellID:0

frequencyInfo:

modeSpecificInfo:

fdd: (FrequencyInfoFDD)

uarfcn_UL (UARFCN):9613
uarfcn_DL (UARFCN):10563

cellInfo: (CellInfoSI_RSCP)

cellIndividualOffset: Omit

referenceTimeDifferenceToCell: Omit

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode:100

primaryCPICH_TX_Power: Omit
readSFN_Indicator:false
tx_DiversityIndicator:false

cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP)

q_OffsetS_N:0
maxAllowedUL_TX_Power:21

modeSpecificInfo:

fdd:

q_QualMin:-16
q_RxlevMin:-58

NewInterFreqCellSI_RSCP:

interFreqCellID:1

frequencyInfo: Omit

cellInfo: (CellInfoSI_RSCP)

cellIndividualOffset: Omit

referenceTimeDifferenceToCell: Omit

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode:150

primaryCPICH_TX_Power: Omit
readSFN_Indicator:false
tx_DiversityIndicator:false

cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP)

q_OffsetS_N:0
maxAllowedUL_TX_Power:21

modeSpecificInfo:

fdd:

q_QualMin:-16
q_RxlevMin:-58

NewInterFreqCellSI_RSCP:

interFreqCellID:2

frequencyInfo: Omit

cellInfo: (CellInfoSI_RSCP)

cellIndividualOffset: Omit

referenceTimeDifferenceToCell: Omit

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode:200

primaryCPICH_TX_Power: Omit
readSFN_Indicator:false
tx_DiversityIndicator:false

cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP)

q_OffsetS_N:0
maxAllowedUL_TX_Power:21

modeSpecificInfo:

fdd:

q_QualMin:-16
q_RxlevMin:-58

NewInterFreqCellSI_RSCP:

interFreqCellID:4

frequencyInfo:

modeSpecificInfo:

fdd: (FrequencyInfoFDD)

uarfcn_UL (UARFCN):9713
uarfcn_DL (UARFCN):10663

cellInfo: (CellInfoSI_RSCP)

cellIndividualOffset: Omit

referenceTimeDifferenceToCell: Omit

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode:150

primaryCPICH_TX_Power: Omit
readSFN_Indicator:false
tx_DiversityIndicator:false

cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP)

q_OffsetS_N:0
maxAllowedUL_TX_Power:21

modeSpecificInfo:

fdd:

q_QualMin:-16
q_RxlevMin:-58

NewInterFreqCellSI_RSCP:

interFreqCellID:7

frequencyInfo: Omit

cellInfo: (CellInfoSI_RSCP)

cellIndividualOffset: Omit

referenceTimeDifferenceToCell: Omit

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode:450

primaryCPICH_TX_Power: Omit
readSFN_Indicator:false
tx_DiversityIndicator:false

cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP)

q_OffsetS_N:0
maxAllowedUL_TX_Power:21

modeSpecificInfo:

fdd:

q_QualMin:-16
q_RxlevMin:-58

interRATMeasurementSysInfo: (InterRATMeasurementSysInfo_B) Omit

trafficVolumeMeasSysInfo: Omit

dummy: (UE_InternalMeasurementSysInfo) Omit

nonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]00 10 00 00 11 01 10 01
[8]00 00 10 10 00 11 00 00
[16]10 01 10 01 00 00 01 00
[24]10 00 01 01 01 00 10 11
[32]00 10 01 10 00 11 10 01
[40]10 10 00 00 00 00 10 01
[48]01 00 10 10 10 10 11 11
[56]01 00 11 00 01 11 00 11
[64]01 00 00 00 00 00 00 10
[72]00 10 00 10 00 11 00 10
[80]01 01 01 01 00 00 00 01
[88]00 10 10 00 01 01 00 10
[96]10 10 00 01 10 00 01 00
[104]10 10 00 10 00 00 10 10
[112]00 01 00 00 11 00 00 10
[120]01 01 00 10 01 10 10 10
[128]10 00 01 10 00 01 00 10
[136]10 10 01 00 11 00 00 00
[144]11 00 10 11 00 01 10 11
[152]01 00 10 10 00 01 10 01
[160]01 00 01 10 01 00 00 01
[168]10 00 11 10 01 10 10 00
[176]00 00 00 10 00 00 10 01
[184]01 00 10 01 01 10 00 01
[192]10 00 11 10 01 10 10 00
[200]00 00 00 10 00 01 00 01
[208]01 00 11 00 10 00 00 01
[216]10 00 11 10 01 10 10 00
[224]00 00 00 11 00 10 00 11
[232]00 10 11 11 10 00 11 01
[240]00 11 01 00 11 10 01 01
[248]00 10 01 01 10 00 01 10
[256]00 11 10 01 10 10 00 00
[264]00 00 10 00 11 10 01 01
[272]01 11 00 00 10 00 01 10
[280]00 11 10 01 10 10 00 00
[288]00 00

#### MAC_DATA_REQ

RLC MAC @ 00:01:09.190

Category: Configuration
BTS unit: 2:1
Channel No: 0 Name: BCCH
CFN: 16

Message Details:

RLC PDU size (bits):16
RLC PDU (raw):

[0]00 00

#### PHY_DATA_REQ

MAC PHY @ 00:01:09.190

BTS unit: 2:1
Channel No: 0 Name: BCH
CFN: 16

Message Details:

SIB repetition period:64
SIB position:14
SIB size:246
SIB (raw):

[0]00 0E 27 17 82 80 81 1B
[8]7A 00 00 00 65 B8 C0 00
[16]80 12 10 23 FF FF F8 86
[24]42 99 0A 00 30 11 14 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 0E 27 17 82 80 81 1B
[8]7A 00 00 00 65 B8 C0 00
[16]80 12 10 23 FF FF F8 86
[24]42 99 0A 00 30 11 14

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:01:09.200

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:3

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:30
bcch_ModificationTime: Omit

#### PHY_DATA_REQ

MAC PHY @ 00:01:09.210

BTS unit: 2:1
Channel No: 0 Name: BCH
CFN: 18

Message Details:

SIB repetition period:64
SIB position:46
SIB size:246
SIB (raw):

[0]00 0E 27 17 82 80 81 D3
[8]14 43 80 08 06 00 20 18
[16]00 80 60 08 21 FF F8 86
[24]42 99 0A 00 30 11 14 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 0E 27 17 82 80 81 D3
[8]14 43 80 08 06 00 20 18
[16]00 80 60 08 21 FF F8 86
[24]42 99 0A 00 30 11 14

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:01:09.220

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:3

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:01:09.220

Channel ID: RbBcch
Cell ID: 3

Message Details:

RLC_TR_DATA_REQ:

cellId:3

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

noSegment:

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:01:09.220

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 60

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

noSegment: NULL

Layer 3 SDU:

[0]00 00

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:01:09.220

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:3

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:27
bcch_ModificationTime: Omit

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:01:09.230

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:3

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:01:09.230

Channel ID: RbBcch
Cell ID: 3

Message Details:

RLC_TR_DATA_REQ:

cellId:3

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

subsequentSegment:

sib_Type:systemInformationBlockType11
segmentIndex:1
sib_Data_fixed:100001000011000010010100100110101010000110000100101010010011000000110010110001101101001010000110010100011001000001100011100110100000000010000010010100100101100001100011100110100000000010000100010100110010000001100011100110

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:01:09.230

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 54

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

subsequentSegment:

sib_Type: systemInformationBlockType11_SIB_Type [enum=11]

segmentIndex: 1

sib_Data_fixed: 100001000011000010010100100110101010000110000100101010010011000000110010110001101101001010000110010100011001000001100011100110100000000010000010010100100101100001100011100110100000000010000100010100110010000001100011100110

Layer 3 SDU:

[0]00 04 B0 84 30 94 9A A1
[8]84 A9 30 32 C6 D2 86 51
[16]90 63 9A 00 82 52 58 63
[24]9A 00 84 53 20 63 98

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:01:09.230

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:3

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:26
bcch_ModificationTime: Omit

#### PHY_DATA_REQ

MAC PHY @ 00:01:09.230

BTS unit: 2:1
Channel No: 0 Name: BCH
CFN: 20

Message Details:

SIB repetition period:64
SIB position:62
SIB size:246
SIB (raw):

[0]00 0E 27 17 82 80 81 22
[8]F0 00 00 00 CB 71 80 01
[16]00 24 00 47 70 FF F8 86
[24]42 99 0A 00 30 11 14 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 0E 27 17 82 80 81 22
[8]F0 00 00 00 CB 71 80 01
[16]00 24 00 47 70 FF F8 86
[24]42 99 0A 00 30 11 14

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:01:09.250

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:3

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:01:09.250

Channel ID: RbBcch
Cell ID: 3

Message Details:

RLC_TR_DATA_REQ:

cellId:3

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

firstSegment:

sib_Type:systemInformationBlockType11
seg_Count (SegCount):3
sib_Data_fixed:001000001101100100001010001100001001100100000100100001010100101100100110001110011010000000001001010010101010111101001100011100110100000000000010001000100011001001010101000000010010100001010010101000011000010010100010000010

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:01:09.250

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 52

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

firstSegment:

sib_Type: systemInformationBlockType11_SIB_Type [enum=11]

seg_Count: 3

sib_Data_fixed: 001000001101100100001010001100001001100100000100100001010100101100100110001110011010000000001001010010101010111101001100011100110100000000000010001000100011001001010101000000010010100001010010101000011000010010100010000010

Layer 3 SDU:

[0]00 02 B2 20 D9 0A 30 99
[8]04 85 4B 26 39 A0 09 4A
[16]AF 4C 73 40 02 22 32 55
[24]01 28 52 A1 84 A2 08

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:01:09.250

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:3

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:29
bcch_ModificationTime: Omit

#### PHY_DATA_REQ

MAC PHY @ 00:01:09.250

BTS unit: 2:1
Channel No: 0 Name: BCH
CFN: 22

Message Details:

SIB repetition period:64
SIB position:60
SIB size:246
SIB (raw):

[0]00 00 27 17 82 80 81 22
[8]F0 00 00 00 CB 71 80 01
[16]00 24 00 47 70 FF F8 86
[24]42 99 0A 00 30 11 14 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 00 27 17 82 80 81 22
[8]F0 00 00 00 CB 71 80 01
[16]00 24 00 47 70 FF F8 86
[24]42 99 0A 00 30 11 14

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:01:09.260

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:3

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:01:09.260

Channel ID: RbBcch
Cell ID: 3

Message Details:

RLC_TR_DATA_REQ:

cellId:3

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

lastSegmentShort:

sib_Type:systemInformationBlockType11
segmentIndex:2
sib_Data_variable:1000000000110010001100101111100011010011010011100101001001011000011000111001101000000000100011100101011100001000011000111001101000000000

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:01:09.260

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 58

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

lastSegmentShort:

sib_Type: systemInformationBlockType11_SIB_Type [enum=11]

segmentIndex: 2

sib_Data_variable: 1000000000110010001100101111100011010011010011100101001001011000011000111001101000000000100011100101011100001000011000111001101000000000

Layer 3 SDU:

[0]00 06 B1 87 80 32 32 F8
[8]D3 4E 52 58 63 9A 00 8E
[16]57 08 63 9A 00

#### o_SIB_PER_Encoding

RRC RRC @ 00:01:09.260

Category: TSO

Message Details:

Inputs:

SIB:

sIB12: (SysInfoType12)

fach_MeasurementOccasionInfo: Omit

measurementControlSysInfo:

use_of_HCS:

hcs_not_used:

cellSelectQualityMeasure:

cpich_RSCP:

intraFreqMeasurementSysInfo: (IntraFreqMeasurementSysInfo_RSCP)

intraFreqMeasurementID (MeasurementIdentity): Omit

intraFreqCellInfoSI_List: (IntraFreqCellInfoSI_List_RSCP)

removedIntraFreqCellList: Omit

newIntraFreqCellList: (NewIntraFreqCellSI_List_RSCP)

NewIntraFreqCellSI_RSCP:

intraFreqCellID:4

cellInfo: (CellInfoSI_RSCP)

cellIndividualOffset: Omit

referenceTimeDifferenceToCell: Omit

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode:300

primaryCPICH_TX_Power: Omit
readSFN_Indicator:true
tx_DiversityIndicator:false

cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP)

q_OffsetS_N:0
maxAllowedUL_TX_Power:21

modeSpecificInfo:

fdd:

q_QualMin:-16
q_RxlevMin:-58

NewIntraFreqCellSI_RSCP:

intraFreqCellID:5

cellInfo: (CellInfoSI_RSCP)

cellIndividualOffset: Omit

referenceTimeDifferenceToCell: Omit

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode:350

primaryCPICH_TX_Power: Omit
readSFN_Indicator:true
tx_DiversityIndicator:false

cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP)

q_OffsetS_N:0
maxAllowedUL_TX_Power:21

modeSpecificInfo:

fdd:

q_QualMin:-16
q_RxlevMin:-58

intraFreqMeasQuantity:

filterCoefficient: Omit

modeSpecificInfo:

fdd:

intraFreqMeasQuantity_FDD:cpich_RSCP

intraFreqReportingQuantityForRACH: Omit

maxReportedCellsOnRACH: Omit

reportingInfoForCellDCH:

intraFreqReportingQuantity:

activeSetReportingQuantities: (CellReportingQuantities)

dummy (SFN_SFN_OTD_Type):noReport
cellIdentity_reportingIndicator:true
cellSynchronisationInfoReportingIndicator:false

modeSpecificInfo:

fdd:

cpich_Ec_N0_reportingIndicator:false
cpich_RSCP_reportingIndicator:true
pathloss_reportingIndicator:false

monitoredSetReportingQuantities: (CellReportingQuantities)

dummy (SFN_SFN_OTD_Type):noReport
cellIdentity_reportingIndicator:true
cellSynchronisationInfoReportingIndicator:true

modeSpecificInfo:

fdd:

cpich_Ec_N0_reportingIndicator:false
cpich_RSCP_reportingIndicator:true
pathloss_reportingIndicator:false

detectedSetReportingQuantities: (CellReportingQuantities) Omit

measurementReportingMode:

measurementReportTransferMode (TransferMode):acknowledgedModeRLC
periodicalOrEventTrigger:eventTrigger

reportCriteria: (CellDCH_ReportCriteria)

intraFreqReportingCriteria:

eventCriteriaList: (IntraFreqEventCriteriaList)

IntraFreqEventCriteria:

event: (IntraFreqEvent)

e1a: (Event1a)

triggeringCondition (TriggeringCondition2):monitoredSetCellsOnly
reportingRange:5

forbiddenAffectCellList: Omit

w:1
reportDeactivationThreshold:t2
reportingAmount:ra4
reportingInterval:noPeriodicalreporting

hysteresis:0
timeToTrigger:ttt640

reportingCellStatus:

withinActiveAndOrMonitoredUsedFreq (MaxNumberOfReportingCellsType1):e3

IntraFreqEventCriteria:

event: (IntraFreqEvent)

e1b: (Event1b)

triggeringCondition (TriggeringCondition1):activeSetCellsOnly
reportingRange:5

forbiddenAffectCellList: Omit

w:1

hysteresis:0
timeToTrigger:ttt640

reportingCellStatus:

withinActiveAndOrMonitoredUsedFreq (MaxNumberOfReportingCellsType1):e3

IntraFreqEventCriteria:

event: (IntraFreqEvent)

e1c: (Event1c)

replacementActivationThreshold:t3
reportingAmount:ra4
reportingInterval:ri4

hysteresis:0
timeToTrigger:ttt640

reportingCellStatus:

withinActiveAndOrMonitoredUsedFreq (MaxNumberOfReportingCellsType1):e3

interFreqMeasurementSysInfo: (InterFreqMeasurementSysInfo_RSCP)

interFreqCellInfoSI_List: (InterFreqCellInfoSI_List_RSCP)

removedInterFreqCellList: Omit

newInterFreqCellList: (NewInterFreqCellSI_List_RSCP)

NewInterFreqCellSI_RSCP:

interFreqCellID:0

frequencyInfo:

modeSpecificInfo:

fdd: (FrequencyInfoFDD)

uarfcn_UL (UARFCN):9613
uarfcn_DL (UARFCN):10563

cellInfo: (CellInfoSI_RSCP)

cellIndividualOffset: Omit

referenceTimeDifferenceToCell: Omit

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode:100

primaryCPICH_TX_Power: Omit
readSFN_Indicator:true
tx_DiversityIndicator:false

cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP)

q_OffsetS_N:0
maxAllowedUL_TX_Power:21

modeSpecificInfo:

fdd:

q_QualMin:-16
q_RxlevMin:-58

NewInterFreqCellSI_RSCP:

interFreqCellID:1

frequencyInfo: Omit

cellInfo: (CellInfoSI_RSCP)

cellIndividualOffset: Omit

referenceTimeDifferenceToCell: Omit

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode:150

primaryCPICH_TX_Power: Omit
readSFN_Indicator:true
tx_DiversityIndicator:false

cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP)

q_OffsetS_N:0
maxAllowedUL_TX_Power:21

modeSpecificInfo:

fdd:

q_QualMin:-16
q_RxlevMin:-58

NewInterFreqCellSI_RSCP:

interFreqCellID:2

frequencyInfo: Omit

cellInfo: (CellInfoSI_RSCP)

cellIndividualOffset: Omit

referenceTimeDifferenceToCell: Omit

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode:200

primaryCPICH_TX_Power: Omit
readSFN_Indicator:true
tx_DiversityIndicator:false

cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP)

q_OffsetS_N:0
maxAllowedUL_TX_Power:21

modeSpecificInfo:

fdd:

q_QualMin:-16
q_RxlevMin:-58

NewInterFreqCellSI_RSCP:

interFreqCellID:4

frequencyInfo:

modeSpecificInfo:

fdd: (FrequencyInfoFDD)

uarfcn_UL (UARFCN):9713
uarfcn_DL (UARFCN):10663

cellInfo: (CellInfoSI_RSCP)

cellIndividualOffset: Omit

referenceTimeDifferenceToCell: Omit

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode:150

primaryCPICH_TX_Power: Omit
readSFN_Indicator:true
tx_DiversityIndicator:false

cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP)

q_OffsetS_N:0
maxAllowedUL_TX_Power:21

modeSpecificInfo:

fdd:

q_QualMin:-16
q_RxlevMin:-58

NewInterFreqCellSI_RSCP:

interFreqCellID:7

frequencyInfo: Omit

cellInfo: (CellInfoSI_RSCP)

cellIndividualOffset: Omit

referenceTimeDifferenceToCell: Omit

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode:450

primaryCPICH_TX_Power: Omit
readSFN_Indicator:true
tx_DiversityIndicator:false

cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP)

q_OffsetS_N:0
maxAllowedUL_TX_Power:21

modeSpecificInfo:

fdd:

q_QualMin:-16
q_RxlevMin:-58

interRATMeasurementSysInfo: (InterRATMeasurementSysInfo_B) Omit

trafficVolumeMeasSysInfo: Omit

dummy: (UE_InternalMeasurementSysInfo) Omit

nonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]00 00 00 01 10 11 00 10
[8]00 00 11 00 10 00 01 01
[16]01 00 10 11 00 10 01 10
[24]00 11 10 01 10 10 00 00
[32]00 00 10 01 01 00 10 10
[40]10 10 11 11 01 00 11 00
[48]01 11 00 11 01 00 00 00
[56]00 00 00 10 00 10 00 10
[64]00 11 00 10 01 01 01 01
[72]00 00 00 01 00 10 10 00
[80]01 01 00 10 00 00 00 01
[88]10 00 01 00 10 10 00 10
[96]00 00 10 10 00 01 00 00
[104]11 00 00 10 01 01 00 10
[112]01 10 10 10 10 00 01 10
[120]00 01 00 10 10 10 01 00
[128]11 00 00 00 11 00 10 11
[136]00 01 10 11 01 00 10 10
[144]00 01 10 01 01 00 01 10
[152]01 00 10 01 10 00 11 10
[160]01 10 10 00 00 00 00 10
[168]00 00 10 01 01 00 10 01
[176]01 10 10 01 10 00 11 10
[184]01 10 10 00 00 00 00 10
[192]00 01 00 01 01 00 11 00
[200]10 00 10 01 10 00 11 10
[208]01 10 10 00 00 00 00 11
[216]00 10 00 11 00 10 11 11
[224]10 00 11 01 00 11 01 00
[232]11 10 01 01 00 10 01 01
[240]10 10 01 10 00 11 10 01
[248]10 10 00 00 00 00 10 00
[256]11 10 01 01 01 11 00 00
[264]10 10 01 10 00 11 10 01
[272]10 10 00 00 00 00

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:01:09.290

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:3

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:13
bcch_ModificationTime: Omit

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:01:09.310

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:3

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:01:09.310

Channel ID: RbBcch
Cell ID: 3

Message Details:

RLC_TR_DATA_REQ:

cellId:3

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

subsequentSegment:

sib_Type:systemInformationBlockType12
segmentIndex:1
sib_Data_fixed:100110101010000110000100101010010011000000110010110001101101001010000110010100011001001001100011100110100000000010000010010100100101101001100011100110100000000010000100010100110010001001100011100110100000000011001000110010

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:01:09.310

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 26

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

subsequentSegment:

sib_Type: systemInformationBlockType12_SIB_Type [enum=12]

segmentIndex: 1

sib_Data_fixed: 100110101010000110000100101010010011000000110010110001101101001010000110010100011001001001100011100110100000000010000010010100100101101001100011100110100000000010000100010100110010001001100011100110100000000011001000110010

Layer 3 SDU:

[0]00 04 C0 9A A1 84 A9 30
[8]32 C6 D2 86 51 92 63 9A
[16]00 82 52 5A 63 9A 00 84
[24]53 22 63 9A 00 C8 C8

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:01:09.310

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:3

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:11
bcch_ModificationTime: Omit

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:01:09.330

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:3

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:01:09.330

Channel ID: RbBcch
Cell ID: 3

Message Details:

RLC_TR_DATA_REQ:

cellId:3

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

firstSegment:

sib_Type:systemInformationBlockType12
seg_Count (SegCount):3
sib_Data_fixed:000000011011001000001100100001010100101100100110001110011010000000001001010010101010111101001100011100110100000000000010001000100011001001010101000000010010100001010010000000011000010010100010000010100001000011000010010100

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:01:09.330

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 22

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

firstSegment:

sib_Type: systemInformationBlockType12_SIB_Type [enum=12]

seg_Count: 3

sib_Data_fixed: 000000011011001000001100100001010100101100100110001110011010000000001001010010101010111101001100011100110100000000000010001000100011001001010101000000010010100001010010000000011000010010100010000010100001000011000010010100

Layer 3 SDU:

[0]00 02 C2 01 B2 0C 85 4B
[8]26 39 A0 09 4A AF 4C 73
[16]40 02 22 32 55 01 28 52
[24]01 84 A2 0A 10 C2 50

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:01:09.330

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:3

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:15
bcch_ModificationTime: Omit

#### MAC_DATA_REQ

RLC MAC @ 00:01:09.330

Category: Configuration
BTS unit: 2:1
Channel No: 0 Name: BCCH
CFN: 30

Message Details:

RLC PDU size (bits):248
RLC PDU (raw):

[0]00 04 B0 84 30 94 9A A1
[8]84 A9 30 32 C6 D2 86 51
[16]90 63 9A 00 82 52 58 63
[24]9A 00 84 53 20 63 98

#### MAC_DATA_REQ

RLC MAC @ 00:01:09.330

Category: Configuration
BTS unit: 2:1
Channel No: 0 Name: BCCH
CFN: 30

Message Details:

RLC PDU size (bits):248
RLC PDU (raw):

[0]00 02 B2 20 D9 0A 30 99
[8]04 85 4B 26 39 A0 09 4A
[16]AF 4C 73 40 02 22 32 55
[24]01 28 52 A1 84 A2 08

#### MAC_DATA_REQ

RLC MAC @ 00:01:09.330

Category: Configuration
BTS unit: 2:1
Channel No: 0 Name: BCCH
CFN: 30

Message Details:

RLC PDU size (bits):168
RLC PDU (raw):

[0]00 06 B1 87 80 32 32 F8
[8]D3 4E 52 58 63 9A 00 8E
[16]57 08 63 9A 00

#### MAC_DATA_REQ

RLC MAC @ 00:01:09.330

Category: Configuration
BTS unit: 2:1
Channel No: 0 Name: BCCH
CFN: 30

Message Details:

RLC PDU size (bits):248
RLC PDU (raw):

[0]00 04 C0 9A A1 84 A9 30
[8]32 C6 D2 86 51 92 63 9A
[16]00 82 52 5A 63 9A 00 84
[24]53 22 63 9A 00 C8 C8

#### MAC_DATA_REQ

RLC MAC @ 00:01:09.330

Category: Configuration
BTS unit: 2:1
Channel No: 0 Name: BCCH
CFN: 30

Message Details:

RLC PDU size (bits):248
RLC PDU (raw):

[0]00 02 C2 01 B2 0C 85 4B
[8]26 39 A0 09 4A AF 4C 73
[16]40 02 22 32 55 01 28 52
[24]01 84 A2 0A 10 C2 50

#### MAC_DATA_REQ

RLC MAC @ 00:01:09.330

Category: Configuration
BTS unit: 2:1
Channel No: 0 Name: BCCH
CFN: 30

Message Details:

RLC PDU size (bits):56
RLC PDU (raw):

[0]00 0E 07 17 82 80 81

#### MAC_DATA_REQ

RLC MAC @ 00:01:09.330

Category: Configuration
BTS unit: 2:1
Channel No: 0 Name: BCCH
CFN: 30

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]00 06 C1 6F F8 D3 4E 52
[8]5A 63 9A 00 8E 57 0A 63
[16]9A 00

#### PHY_DATA_REQ

MAC PHY @ 00:01:09.330

BTS unit: 2:1
Channel No: 0 Name: BCH
CFN: 30

Message Details:

SIB repetition period:64
SIB position:54
SIB size:246
SIB (raw):

[0]00 04 B0 84 30 94 9A A1
[8]84 A9 30 32 C6 D2 86 51
[16]90 63 9A 00 82 52 58 63
[24]9A 00 84 53 20 63 98 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 04 B0 84 30 94 9A A1
[8]84 A9 30 32 C6 D2 86 51
[16]90 63 9A 00 82 52 58 63
[24]9A 00 84 53 20 63 98

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:01:09.340

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:3

routingInfo:

rB_Identity:-1

#### o_SIB_PER_Encoding

RRC RRC @ 00:01:09.340

Category: TSO

Message Details:

Inputs:

SIB:

sIB7: (SysInfoType7)

modeSpecificInfo:

fdd:

ul_Interference:-100

prach_Information_SIB5_List: (DynamicPersistenceLevelList)

DynamicPersistenceLevel:2

prach_Information_SIB6_List: (DynamicPersistenceLevelList)

DynamicPersistenceLevel:2

expirationTimeFactor: Omit

nonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]10 00 00 10 10 00 00 00
[8]10 00 00 01

#### RLC_TR_DATA_REQ

RRC LLA @ 00:01:09.340

Channel ID: RbBcch
Cell ID: 3

Message Details:

RLC_TR_DATA_REQ:

cellId:3

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

completeSIB_List:

CompleteSIBshort:

sib_Type:systemInformationBlockType7
sib_Data_variable:100000101000000010000001

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:01:09.340

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 30

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

completeSIB_List:

CompleteSIB_List.element:

sib_Type: systemInformationBlockType7_SIB_Type [enum=7]

sib_Data_variable: 100000101000000010000001

Layer 3 SDU:

[0]00 0E 07 17 82 80 81

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:01:09.340

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:3

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:14
bcch_ModificationTime: Omit

#### PHY_DATA_REQ

MAC PHY @ 00:01:09.350

BTS unit: 2:1
Channel No: 0 Name: BCH
CFN: 32

Message Details:

SIB repetition period:64
SIB position:52
SIB size:246
SIB (raw):

[0]00 02 B2 20 D9 0A 30 99
[8]04 85 4B 26 39 A0 09 4A
[16]AF 4C 73 40 02 22 32 55
[24]01 28 52 A1 84 A2 08 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 02 B2 20 D9 0A 30 99
[8]04 85 4B 26 39 A0 09 4A
[16]AF 4C 73 40 02 22 32 55
[24]01 28 52 A1 84 A2 08

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:01:09.360

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:3

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:01:09.360

Channel ID: RbBcch
Cell ID: 3

Message Details:

RLC_TR_DATA_REQ:

cellId:3

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

lastSegmentShort:

sib_Type:systemInformationBlockType12
segmentIndex:2
sib_Data_variable:1111100011010011010011100101001001011010011000111001101000000000100011100101011100001010011000111001101000000000

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:01:09.360

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 28

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

lastSegmentShort:

sib_Type: systemInformationBlockType12_SIB_Type [enum=12]

segmentIndex: 2

sib_Data_variable: 1111100011010011010011100101001001011010011000111001101000000000100011100101011100001010011000111001101000000000

Layer 3 SDU:

[0]00 06 C1 6F F8 D3 4E 52
[8]5A 63 9A 00 8E 57 0A 63
[16]9A 00

#### o_SIB_PER_Encoding

RRC RRC @ 00:01:09.360

Category: TSO

Message Details:

Inputs:

SIB:

sIB18: (SysInfoType18)

idleModePLMNIdentities: (PLMNIdentitiesOfNeighbourCells)

plmnsOfIntraFreqCellsList: Omit

plmnsOfInterFreqCellsList:

:

plmn_Identity:

mcc:

Digit:0
Digit:0
Digit:1

mnc:

Digit:0
Digit:1

:

plmn_Identity:

mcc:

Digit:0
Digit:0
Digit:1

mnc:

Digit:0
Digit:1

:

plmn_Identity:

mcc:

Digit:0
Digit:0
Digit:1

mnc:

Digit:0
Digit:1

:

plmn_Identity:

mcc:

Digit:0
Digit:0
Digit:4

mnc:

Digit:2
Digit:1

plmnsOfInterRATCellsList: Omit

connectedModePLMNIdentities: (PLMNIdentitiesOfNeighbourCells) Omit

nonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]10 00 10 00 01 11 00 00
[8]00 00 00 01 00 00 00 00
[16]11 00 00 00 00 00 01 00
[24]00 00 00 11 00 00 00 00
[32]00 01 00 00 00 00 11 00
[40]00 00 00 01 00 00 01 00
[48]00 1

#### o_SIB_PER_Encoding

RRC RRC @ 00:01:09.360

Category: TSO

Message Details:

Inputs:

SIB:

sIB7: (SysInfoType7)

modeSpecificInfo:

fdd:

ul_Interference:-100

prach_Information_SIB5_List: (DynamicPersistenceLevelList)

DynamicPersistenceLevel:2

prach_Information_SIB6_List: (DynamicPersistenceLevelList)

DynamicPersistenceLevel:2

expirationTimeFactor: Omit

nonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]10 00 00 10 10 00 00 00
[8]10 00 00 01

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:01:09.360

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:3

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:23
bcch_ModificationTime: Omit

#### MAC_DATA_REQ

RLC MAC @ 00:01:09.360

Category: Configuration
BTS unit: 2:1
Channel No: 0 Name: BCCH
CFN: 33

Message Details:

RLC PDU size (bits):168
RLC PDU (raw):

[0]00 0E 27 17 82 80 81 D3
[8]14 43 80 08 06 00 20 18
[16]00 80 60 08 21

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:01:09.370

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:3

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:01:09.370

Channel ID: RbBcch
Cell ID: 3

Message Details:

RLC_TR_DATA_REQ:

cellId:3

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

completeSIB_List:

CompleteSIBshort:

sib_Type:systemInformationBlockType7
sib_Data_variable:100000101000000010000001

CompleteSIBshort:

sib_Type:systemInformationBlockType18
sib_Data_variable:100010000111000000000001000000001100000000000100000000110000000000010000000011000000000100000100001

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:01:09.370

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 46

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

completeSIB_List:

CompleteSIB_List.element:

sib_Type: systemInformationBlockType7_SIB_Type [enum=7]

sib_Data_variable: 100000101000000010000001

CompleteSIB_List.element:

sib_Type: systemInformationBlockType18_SIB_Type [enum=26]

sib_Data_variable: 100010000111000000000001000000001100000000000100000000110000000000010000000011000000000100000100001

Layer 3 SDU:

[0]00 0E 27 17 82 80 81 D3
[8]14 43 80 08 06 00 20 18
[16]00 80 60 08 21

#### o_SIB_PER_Encoding

RRC RRC @ 00:01:09.370

Category: TSO

Message Details:

Inputs:

SIB:

sB1: (SysInfoTypeSB1)

sib_ReferenceList:

SchedulingInformationSIB:

sib_Type: (SIB_TypeAndTag)

sysInfoType6 (CellValueTag):2

scheduling: (SchedulingInformation)

scheduling:

segCount: Omit

sib_Pos:

rep64:2

sib_PosOffsetInfo: (SibOFF_List) Omit

SchedulingInformationSIB:

sib_Type: (SIB_TypeAndTag)

sysInfoType7:

scheduling: (SchedulingInformation)

scheduling:

segCount: Omit

sib_Pos:

rep16:7

sib_PosOffsetInfo: (SibOFF_List) Omit

SchedulingInformationSIB:

sib_Type: (SIB_TypeAndTag)

sysInfoType11 (CellValueTag):2

scheduling: (SchedulingInformation)

scheduling:

segCount:3

sib_Pos:

rep64:26

sib_PosOffsetInfo: (SibOFF_List)

SibOFF:so2
SibOFF:so4

SchedulingInformationSIB:

sib_Type: (SIB_TypeAndTag)

sysInfoType12 (CellValueTag):2

scheduling: (SchedulingInformation)

scheduling:

segCount:3

sib_Pos:

rep64:11

sib_PosOffsetInfo: (SibOFF_List)

SibOFF:so4
SibOFF:so2

SchedulingInformationSIB:

sib_Type: (SIB_TypeAndTag)

sysInfoType18 (CellValueTag):2

scheduling: (SchedulingInformation)

scheduling:

segCount: Omit

sib_Pos:

rep64:23

sib_PosOffsetInfo: (SibOFF_List) Omit

nonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]00 01 00 00 10 10 10 00
[8]10 00 00 10 00 11 00 00
[16]01 01 11 01 01 00 11 10
[24]01 00 10 01 10 10 00 01
[32]00 00 00 01 01 01 10 11
[40]10 01 00 10 00 10 11 00
[48]01 00 01 00 00 11 00 10
[56]10 00 10 01 01 11

#### PHY_DATA_REQ

MAC PHY @ 00:01:09.370

BTS unit: 2:1
Channel No: 0 Name: BCH
CFN: 34

Message Details:

SIB repetition period:64
SIB position:58
SIB size:246
SIB (raw):

[0]00 06 B1 87 80 32 32 F8
[8]D3 4E 52 58 63 9A 00 8E
[16]57 08 63 9A 00 22 32 55
[24]01 28 52 A1 84 A2 08 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 06 B1 87 80 32 32 F8
[8]D3 4E 52 58 63 9A 00 8E
[16]57 08 63 9A 00 22 32 55
[24]01 28 52 A1 84 A2 08

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:01:09.390

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:3

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:4
sg_POS:1
bcch_ModificationTime: Omit

#### PHY_DATA_REQ

MAC PHY @ 00:01:09.390

BTS unit: 2:1
Channel No: 0 Name: BCH
CFN: 36

Message Details:

SIB repetition period:64
SIB position:26
SIB size:246
SIB (raw):

[0]00 04 C0 9A A1 84 A9 30
[8]32 C6 D2 86 51 92 63 9A
[16]00 82 52 5A 63 9A 00 84
[24]53 22 63 9A 00 C8 C8 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 04 C0 9A A1 84 A9 30
[8]32 C6 D2 86 51 92 63 9A
[16]00 82 52 5A 63 9A 00 84
[24]53 22 63 9A 00 C8 C8

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:01:09.400

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:3

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:01:09.400

Channel ID: RbBcch
Cell ID: 3

Message Details:

RLC_TR_DATA_REQ:

cellId:3

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

completeSIB_List:

CompleteSIBshort:

sib_Type:schedulingBlock1
sib_Data_variable:0001000010101000100000100011000001011101010011100100100110100001000000010101101110010010001011000100010000110010100010010111

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:01:09.400

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 16

SIB position: 2

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

completeSIB_List:

CompleteSIB_List.element:

sib_Type: schedulingBlock1_SIB_Type [enum=27]

sib_Data_variable: 0001000010101000100000100011000001011101010011100100100110100001000000010101101110010010001011000100010000110010100010010111

Layer 3 SDU:

[0]00 0E 1B 7B 10 A8 82 30
[8]5D 4E 49 A1 01 5B 92 2C
[16]44 32 89 70

#### o_SIB_PER_Encoding

RRC RRC @ 00:01:09.400

Category: TSO

Message Details:

Inputs:

SIB:

mIB: (MasterInformationBlock)

mib_ValueTag:2

plmn_Type:

gsm_MAP:

plmn_Identity:

mcc:

Digit:0
Digit:0
Digit:2

mnc:

Digit:1
Digit:1

sibSb_ReferenceList:

SchedulingInformationSIBSb:

sibSb_Type: (SIBSb_TypeAndTag)

sysInfoTypeSB1 (CellValueTag):2

scheduling: (SchedulingInformation)

scheduling:

segCount: Omit

sib_Pos:

rep16:1

sib_PosOffsetInfo: (SibOFF_List) Omit

SchedulingInformationSIBSb:

sibSb_Type: (SIBSb_TypeAndTag)

sysInfoType1 (PLMN_ValueTag):2

scheduling: (SchedulingInformation)

scheduling:

segCount: Omit

sib_Pos:

rep64:10

sib_PosOffsetInfo: (SibOFF_List) Omit

SchedulingInformationSIBSb:

sibSb_Type: (SIBSb_TypeAndTag)

sysInfoType2 (CellValueTag):2

scheduling: (SchedulingInformation)

scheduling:

segCount: Omit

sib_Pos:

rep64:10

sib_PosOffsetInfo: (SibOFF_List) Omit

SchedulingInformationSIBSb:

sibSb_Type: (SIBSb_TypeAndTag)

sysInfoType3 (CellValueTag):2

scheduling: (SchedulingInformation)

scheduling:

segCount: Omit

sib_Pos:

rep64:7

sib_PosOffsetInfo: (SibOFF_List) Omit

SchedulingInformationSIBSb:

sibSb_Type: (SIBSb_TypeAndTag)

sysInfoType4 (CellValueTag):2

scheduling: (SchedulingInformation)

scheduling:

segCount: Omit

sib_Pos:

rep64:31

sib_PosOffsetInfo: (SibOFF_List) Omit

SchedulingInformationSIBSb:

sibSb_Type: (SIBSb_TypeAndTag)

sysInfoType5 (CellValueTag):2

scheduling: (SchedulingInformation)

scheduling:

segCount:3

sib_Pos:

rep64:18

sib_PosOffsetInfo: (SibOFF_List)

SibOFF:so2
SibOFF:so4

nonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]00 01 00 00 00 00 00 00
[8]10 00 00 10 00 10 01 01
[16]10 10 10 10 00 01 00 01
[24]00 00 00 00 00 00 10 00
[32]10 00 10 10 00 00 10 10
[40]00 10 00 10 10 00 01 00
[48]10 00 10 00 01 11 00 01
[56]10 10 00 10 01 11 11 00
[64]10 00 11 10 01 00 10 01
[72]00 10 00 01 00 00 00 01

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:01:09.400

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:3

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:3
sg_POS:0
bcch_ModificationTime: Omit

#### PHY_DATA_REQ

MAC PHY @ 00:01:09.410

BTS unit: 2:1
Channel No: 0 Name: BCH
CFN: 38

Message Details:

SIB repetition period:64
SIB position:22
SIB size:246
SIB (raw):

[0]00 02 C2 01 B2 0C 85 4B
[8]26 39 A0 09 4A AF 4C 73
[16]40 02 22 32 55 01 28 52
[24]01 84 A2 0A 10 C2 50 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 02 C2 01 B2 0C 85 4B
[8]26 39 A0 09 4A AF 4C 73
[16]40 02 22 32 55 01 28 52
[24]01 84 A2 0A 10 C2 50

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:01:09.420

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:3

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:01:09.420

Channel ID: RbBcch
Cell ID: 3

Message Details:

RLC_TR_DATA_REQ:

cellId:3

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

completeSIB_List:

CompleteSIBshort:

sib_Type:masterInformationBlock
sib_Data_variable:0001000000000000100000100010010110101010000100010000000000001000100010100000101000100010100001001000100001110001101000100111110010001110010010010010000100000001

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:01:09.420

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 8

SIB position: 0

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

completeSIB_List:

CompleteSIB_List.element:

sib_Type: masterInformationBlock_SIB_Type [enum=0]

sib_Data_variable: 0001000000000000100000100010010110101010000100010000000000001000100010100000101000100010100001001000100001110001101000100111110010001110010010010010000100000001

Layer 3 SDU:

[0]00 0E 00 9F 10 00 82 25
[8]AA 11 00 08 8A 0A 22 84
[16]88 71 A2 7C 8E 49 21 01

#### PHY_DATA_REQ

MAC PHY @ 00:01:09.430

BTS unit: 2:1
Channel No: 0 Name: BCH
CFN: 40

Message Details:

SIB repetition period:64
SIB position:30
SIB size:246
SIB (raw):

[0]00 0E 07 17 82 80 81 4B
[8]26 39 A0 09 4A AF 4C 73
[16]40 02 22 32 55 01 28 52
[24]01 84 A2 0A 10 C2 50 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 0E 07 17 82 80 81 4B
[8]26 39 A0 09 4A AF 4C 73
[16]40 02 22 32 55 01 28 52
[24]01 84 A2 0A 10 C2 50

#### PHY_DATA_REQ

MAC PHY @ 00:01:09.450

BTS unit: 2:1
Channel No: 0 Name: BCH
CFN: 42

Message Details:

SIB repetition period:64
SIB position:28
SIB size:246
SIB (raw):

[0]00 06 C1 6F F8 D3 4E 52
[8]5A 63 9A 00 8E 57 0A 63
[16]9A 00 22 32 55 01 28 52
[24]01 84 A2 0A 10 C2 50 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 06 C1 6F F8 D3 4E 52
[8]5A 63 9A 00 8E 57 0A 63
[16]9A 00 22 32 55 01 28 52
[24]01 84 A2 0A 10 C2 50

#### PHY_DATA_REQ

MAC PHY @ 00:01:09.470

BTS unit: 2:1
Channel No: 0 Name: BCH
CFN: 44

Message Details:

SIB repetition period:64
SIB position:46
SIB size:246
SIB (raw):

[0]00 0E 27 17 82 80 81 D3
[8]14 43 80 08 06 00 20 18
[16]00 80 60 08 21 01 28 52
[24]01 84 A2 0A 10 C2 50 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 0E 27 17 82 80 81 D3
[8]14 43 80 08 06 00 20 18
[16]00 80 60 08 21 01 28 52
[24]01 84 A2 0A 10 C2 50

#### MAC_DATA_REQ

RLC MAC @ 00:01:09.510

Category: Configuration
BTS unit: 2:1
Channel No: 0 Name: BCCH
CFN: 48

Message Details:

RLC PDU size (bits):160
RLC PDU (raw):

[0]00 0E 1B 7B 10 A8 82 30
[8]5D 4E 49 A1 01 5B 92 2C
[16]44 32 89 70

#### MAC_DATA_REQ

RLC MAC @ 00:01:09.510

Category: Configuration
BTS unit: 2:1
Channel No: 0 Name: BCCH
CFN: 48

Message Details:

RLC PDU size (bits):192
RLC PDU (raw):

[0]00 0E 00 9F 10 00 82 25
[8]AA 11 00 08 8A 0A 22 84
[16]88 71 A2 7C 8E 49 21 01

#### PHY_DATA_REQ

MAC PHY @ 00:01:09.510

BTS unit: 2:1
Channel No: 0 Name: BCH
CFN: 48

Message Details:

SIB repetition period:16
SIB position:2
SIB size:246
SIB (raw):

[0]00 0E 1B 7B 10 A8 82 30
[8]5D 4E 49 A1 01 5B 92 2C
[16]44 32 89 70 21 01 28 52
[24]01 84 A2 0A 10 C2 50 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 0E 1B 7B 10 A8 82 30
[8]5D 4E 49 A1 01 5B 92 2C
[16]44 32 89 70 21 01 28 52
[24]01 84 A2 0A 10 C2 50

#### PHY_DATA_REQ

MAC PHY @ 00:01:09.530

BTS unit: 2:1
Channel No: 0 Name: BCH
CFN: 50

Message Details:

SIB repetition period:8
SIB position:0
SIB size:246
SIB (raw):

[0]00 0E 00 9F 10 00 82 25
[8]AA 11 00 08 8A 0A 22 84
[16]88 71 A2 7C 8E 49 21 01
[24]01 84 A2 0A 10 C2 50 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 0E 00 9F 10 00 82 25
[8]AA 11 00 08 8A 0A 22 84
[16]88 71 A2 7C 8E 49 21 01
[24]01 84 A2 0A 10 C2 50

#### CMAC Configuration REQ

LLA MAC @ 00:01:14.410

BTS unit: 2:1
Channel No: 0 Name: S_CCPCH
CFN: 26

Message Details:

Configuration Parameters:

Number Of Transport Channels:3

Transport Channels:

Item Number 0:

Transport Channel Parameters:

Transport Channel:

Name:PCH
Identity:0

TTI (ms):10
EP Type:1/2 Rate Convolutional Coding
CRC Size:16
RM Attribute:230
First Interleave:On
Number Of Transport Formats:2

Transport Format Set:

Transport Format 0:

Number Of Transport Blocks:0
Transport Block Size In Bits:240

Transport Format 1:

Number Of Transport Blocks:1
Transport Block Size In Bits:240

Number Of Logical Channels:1

Logical Channels:

Item Number 0:

Logical Channel:

Name:PCCH
Identity:0

Priority:1
CT Length:0
CT Value:0
TCTF Length:0
TCTF Value:0
UE ID Type:Not used
UE ID:0

Item Number 1:

Transport Channel Parameters:

Transport Channel:

Name:FACH
Identity:0

TTI (ms):10
EP Type:1/2 Rate Convolutional Coding
CRC Size:16
RM Attribute:220
First Interleave:On
Number Of Transport Formats:3

Transport Format Set:

Transport Format 0:

Number Of Transport Blocks:0
Transport Block Size In Bits:168

Transport Format 1:

Number Of Transport Blocks:1
Transport Block Size In Bits:168

Transport Format 2:

Number Of Transport Blocks:2
Transport Block Size In Bits:168

Number Of Logical Channels:1

Logical Channels:

Item Number 0:

Logical Channel:

Name:CCCH
Identity:1

Priority:1
CT Length:0
CT Value:0
TCTF Length:8
TCTF Value:64
UE ID Type:Not used
UE ID:0

Item Number 2:

Transport Channel Parameters:

Transport Channel:

Name:FACH
Identity:1

TTI (ms):10
EP Type:Turbo Coding
CRC Size:16
RM Attribute:130
First Interleave:On
Number Of Transport Formats:2

Transport Format Set:

Transport Format 0:

Number Of Transport Blocks:0
Transport Block Size In Bits:360

Transport Format 1:

Number Of Transport Blocks:1
Transport Block Size In Bits:360

Number Of Logical Channels:0

Active Flag:1

Transport Format Combination Set:

Number Of Transport Format Combinations:8

Transport Format Combinations 0:

Transport Format:0
Transport Format:0
Transport Format:0

Transport Format Combinations 1:

Transport Format:1
Transport Format:0
Transport Format:0

Transport Format Combinations 2:

Transport Format:0
Transport Format:1
Transport Format:0

Transport Format Combinations 3:

Transport Format:1
Transport Format:1
Transport Format:0

Transport Format Combinations 4:

Transport Format:0
Transport Format:2
Transport Format:0

Transport Format Combinations 5:

Transport Format:1
Transport Format:2
Transport Format:0

Transport Format Combinations 6:

Transport Format:0
Transport Format:0
Transport Format:1

Transport Format Combinations 7:

Transport Format:0
Transport Format:1
Transport Format:1

#### CMAC_PAGING_Config_REQ

RRC LLA @ 00:01:14.420

Channel ID: S-CCPCH#1
Cell ID: 3

Message Details:

CMAC_PAGING_Config_REQ:

cellId:3

routingInfo:

physicalChannelIdentity:5

ratType:fdd

configMessage: (CmacPagingConfigReq)

pI_BitMapInfo:

e18:000000000000000100

dRX_CycleLength:7

iMSI: (IMSI_GSM_MAP)

Digit:0
Digit:0
Digit:1
Digit:0
Digit:1
Digit:0
Digit:0
Digit:0
Digit:0
Digit:0
Digit:0
Digit:0
Digit:3
Digit:3
Digit:3

t_pich_T_sccpch:false

#### CMAC_PAGING_Config_CNF

LLA RRC @ 00:01:14.440

Channel ID: S-CCPCH#1
Cell ID: 3

Message Details:

CMAC_PAGING_Config_CNF:

cellId:3

routingInfo:

physicalChannelIdentity:5

#### RLC_TR_DATA_REQ

RRC LLA @ 00:01:14.440

Channel ID: RbPcch
Cell ID: 3

Message Details:

RLC_TR_DATA_REQ:

cellId:3

routingInfo:

rB_Identity:-2

tM_message:

pCCH_Message:

message: (PCCH_MessageType)

pagingType1:

pagingRecordList: Omit

bcch_ModificationInfo:

mib_ValueTag:2
bcch_ModificationTime: Omit

laterNonCriticalExtensions: Omit

#### RLC_TR_DATA_REQ: pagingType1

LLA RLC @ 00:01:14.440

Channel No: 0 Name: PCCH

Message Details:

Paging Indicator: 15

DRX Cycle Length: 128

Paging Occasion: 77

PCCH_Message:

message:

pagingType1:

pagingRecordList: Omitted

bcch_ModificationInfo:

mib_ValueTag: 2

bcch_ModificationTime: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]21

#### CPHY_Cell_Config_REQ

RRC LLA @ 00:01:14.440

Cell ID: 6

Message Details:

CPHY_Cell_Config_REQ:

cellId:6
tcell:7253
sfnOffset:1356

frequencyInfo:

modeSpecificInfo:

fdd: (FrequencyInfoFDD)

uarfcn_UL (UARFCN):9713
uarfcn_DL (UARFCN):10663

primaryScramblingCode_SS:150

cellTxPowerLevel:

defaultCellTxPowerLvl:

dLTxAttenuationLevel:8

#### CPHY BTS Frequency REQ

LLA PHY @ 00:01:14.450

BTS unit: 1:2
CFN: 30

Message Details:

Configuration Parameters:

Down Link Frequency:2132600000
Up Link Frequency:1942600000

#### MAC_DATA_REQ

RLC MAC @ 00:01:14.410

Category: Configuration
BTS unit: 2:1
Channel No: 0 Name: PCCH
CFN: 26

Message Details:

RLC PDU size (bits):8
RLC PDU (raw):

[0]21

#### CMAC Configuration CNF

MAC LLA @ 00:01:14.410

BTS unit: 2:1
Channel No: 0 Name: S_CCPCH
CFN: 26

Message Details:

#### CPHY BTS Frequency CNF

PHY LLA @ 00:01:14.450

BTS unit: 1:2
CFN: 30

Message Details:

#### CPHY_Cell_Config_CNF

LLA RRC @ 00:01:14.480

Cell ID: 6

Message Details:

CPHY_Cell_Config_CNF:

cellId:6

#### CPHY_RL_Setup_REQ

RRC LLA @ 00:01:14.480

Channel ID: P-CPICH
Cell ID: 6

Message Details:

CPHY_RL_Setup_REQ:

cellId:6

routingInfo:

physicalChannelIdentity:0

ratType:fdd

setupMessage: (CphyRlSetupReq)

physicalChannelInfo:

primaryCPICHInfo:

dl_TxPower_PCPICH:-60
txdiversityIndicator:false

#### CPHY Radio Link Setup REQ

LLA PHY @ 00:01:14.490

BTS unit: 1:2
Channel No: 0 Name: P_CPICH
CFN: 34

Message Details:

Configuration Parameters:

Channel Offset:7680
Scrambling Code:2400
Symbol Rate:15k
Channelization Code:0
Adjust Time:0
Power in dBm:-48
Tx Diversity:Off
NumOfDpdch:0

#### CPHY Radio Link Setup CNF

PHY LLA @ 00:01:14.490

BTS unit: 1:2
Channel No: 0 Name: P_CPICH
CFN: 34

Message Details:

#### CPHY_RL_Setup_CNF

LLA RRC @ 00:01:14.500

Channel ID: P-CPICH
Cell ID: 6

Message Details:

CPHY_RL_Setup_CNF:

cellId:6

routingInfo:

physicalChannelIdentity:0

#### CPHY_RL_Setup_REQ

RRC LLA @ 00:01:14.500

Channel ID: P-SCH
Cell ID: 6

Message Details:

CPHY_RL_Setup_REQ:

cellId:6

routingInfo:

physicalChannelIdentity:1

ratType:fdd

setupMessage: (CphyRlSetupReq)

physicalChannelInfo:

primarySCHInfo:

tstdIndicator:false
dl_TxPower:-5

#### CPHY Radio Link Setup REQ

LLA PHY @ 00:01:14.510

BTS unit: 1:2
Channel No: 0 Name: P_SCH
CFN: 36

Message Details:

Configuration Parameters:

Channel Offset:7680
Adjust Time:0
Power in dBm:-53
Tx Diversity:Off
NumOfDpdch:0

#### CPHY Radio Link Setup CNF

PHY LLA @ 00:01:14.510

BTS unit: 1:2
Channel No: 0 Name: P_SCH
CFN: 36

Message Details:

#### CPHY_RL_Setup_CNF

LLA RRC @ 00:01:14.530

Channel ID: P-SCH
Cell ID: 6

Message Details:

CPHY_RL_Setup_CNF:

cellId:6

routingInfo:

physicalChannelIdentity:1

#### CPHY_RL_Setup_REQ

RRC LLA @ 00:01:14.530

Channel ID: S-SCH
Cell ID: 6

Message Details:

CPHY_RL_Setup_REQ:

cellId:6

routingInfo:

physicalChannelIdentity:2

ratType:fdd

setupMessage: (CphyRlSetupReq)

physicalChannelInfo:

secondarySCHInfo:

tstdIndicator:false
dl_TxPower:-5

#### CPHY_RL_Setup_CNF

LLA RRC @ 00:01:14.540

Channel ID: S-SCH
Cell ID: 6

Message Details:

CPHY_RL_Setup_CNF:

cellId:6

routingInfo:

physicalChannelIdentity:2

#### CPHY_RL_Setup_REQ

RRC LLA @ 00:01:14.540

Channel ID: P-CCPCH
Cell ID: 6

Message Details:

CPHY_RL_Setup_REQ:

cellId:6

routingInfo:

physicalChannelIdentity:4

ratType:fdd

setupMessage: (CphyRlSetupReq)

physicalChannelInfo:

primaryCCPCHInfo:

sttd_Indicator:false
dl_TxPower:-2

#### CPHY Radio Link Setup REQ

LLA PHY @ 00:01:14.540

BTS unit: 1:2
Channel No: 0 Name: S_SCH
CFN: 39

Message Details:

Configuration Parameters:

Channel Offset:7680
Adjust Time:0
Power in dBm:-53
Tx Diversity:Off
NumOfDpdch:0

#### CPHY Radio Link Setup CNF

PHY LLA @ 00:01:14.540

BTS unit: 1:2
Channel No: 0 Name: S_SCH
CFN: 39

Message Details:

#### CPHY Radio Link Setup REQ

LLA PHY @ 00:01:14.550

BTS unit: 1:2
Channel No: 0 Name: P_CCPCH
CFN: 40

Message Details:

Configuration Parameters:

Channel Offset:7680
SFN Offset:0
Scrambling Code:2400
Symbol Rate:15k
Channelization Code:1
Adjust Time:0
Power in dBm:-50
Tx Diversity:Off
NumOfDpdch:1

#### CPHY Radio Link Setup CNF

PHY LLA @ 00:01:14.550

BTS unit: 1:2
Channel No: 0 Name: P_CCPCH
CFN: 40

Message Details:

#### CPHY_RL_Setup_CNF

LLA RRC @ 00:01:14.560

Channel ID: P-CCPCH
Cell ID: 6

Message Details:

CPHY_RL_Setup_CNF:

cellId:6

routingInfo:

physicalChannelIdentity:4

#### CPHY_TrCH_Config_REQ

RRC LLA @ 00:01:14.560

Channel ID: P-CCPCH
Cell ID: 6

Message Details:

CPHY_TrCH_Config_REQ:

cellId:6

routingInfo:

physicalChannelIdentity:4

ratType:fdd

trchConfigType:

nonDch:

configMessage: (CphyTrchConfigReq)

activationTime: (SS_ActivationTime)

activateNow:

ulconnectedTrCHList: Omit

ulTFCS: (TFCS) Omit

dlconnectedTrCHList:

:

trchid (TransportChannelIdentity):11
dl_TransportChannelType (SS_DL_TransportChannelType):bch

transportChannelInfo: (CommonOrDedicatedTFS)

tti:

tti20: (CommonOrDedicatedTF_InfoList)

CommonOrDedicatedTF_Info:

tb_Size:246

numberOfTbSizeList:

NumberOfTransportBlocks:

one:

logicalChannelList:

configured:

semistaticTF_Information:

channelCodingType:

convolutional (CodingRate):half

rateMatchingAttribute:1
crc_Size:crc16

dlTFCS: (TFCS)

normalTFCI_Signalling: (ExplicitTFCS_Configuration)

complete: (TFCS_ReconfAdd)

ctfcSize:

ctfc2Bit:

:

ctfc2:0

powerOffsetInformation:

gainFactorInformation:

signalledGainFactors:

modeSpecificInfo:

fdd:

gainFactorBetaC (GainFactor):11

gainFactorBetaD (GainFactor):15
referenceTFC_ID:0

powerOffsetPp_m: Omit

#### CPHY_TrCH_Config_CNF

LLA RRC @ 00:01:14.760

Channel ID: P-CCPCH
Cell ID: 6

Message Details:

CPHY_TrCH_Config_CNF:

cellId:6

routingInfo:

physicalChannelIdentity:4

#### CMAC_Config_REQ

RRC LLA @ 00:01:14.760

Channel ID: P-CCPCH
Cell ID: 6

Message Details:

CMAC_Config_REQ:

cellId:6

routingInfo:

physicalChannelIdentity:4

ratType:fdd

configMessage:

setup: (CmacConfigReq)

activationTime: (SS_ActivationTime)

activateNow:

uE_Info:

u_RNTI: Omit

c_RNTI: Omit

trCHInfo:

ulconnectedTrCHList: Omit

ulTFCS: (TFCS) Omit

dlconnectedTrCHList:

:

trchid (TransportChannelIdentity):11

transportChannelInfo: (CommonOrDedicatedTFS)

tti:

tti20: (CommonOrDedicatedTF_InfoList)

CommonOrDedicatedTF_Info:

tb_Size:246

numberOfTbSizeList:

NumberOfTransportBlocks:

one:

logicalChannelList:

configured:

semistaticTF_Information:

channelCodingType:

convolutional (CodingRate):half

rateMatchingAttribute:1
crc_Size:crc16

dlTFCS: (TFCS)

normalTFCI_Signalling: (ExplicitTFCS_Configuration)

complete: (TFCS_ReconfAdd)

ctfcSize:

ctfc2Bit:

:

ctfc2:0

powerOffsetInformation:

gainFactorInformation:

signalledGainFactors:

modeSpecificInfo:

fdd:

gainFactorBetaC (GainFactor):11

gainFactorBetaD (GainFactor):15
referenceTFC_ID:0

powerOffsetPp_m: Omit

trCH_LogCHMapping: (TrCH_LogCHMappingList1)

ulconnectedTrCHList: Omit

dlconnectedTrCHList:

:

trchid (TransportChannelIdentity):11

trCH_LogCHMappingList:

TrCH_LogicalChannelMapping:

logicalChannel_Mapping:

dl_LogicalChannelMapping: (SS_DL_LogicalChannelMapping)

macHeaderManipulation (MAC_HeaderManipulation):normalMacHeader
dl_TransportChannelType (SS_DL_TransportChannelType):bch
logicalChannelIdentity:1
logicalChannelType:bCCH

rlc_SizeList:

configured:

mac_LogicalChannelPriority:1

rB_Identity:-1
cn_DomainIdentity: Omit

#### CPHY Transport Channel Configuration REQ

LLA PHY @ 00:01:14.760

BTS unit: 1:2
Channel No: 0 Name: P_CCPCH
CFN: 61

Message Details:

Configuration Parameters:

DTX Position:Flexible
Second Interleave:On
Puncture Limit:0
CCTrCH Length:270
Number Of Transport Channels:1

Transport Channels:

Item Number 0:

Transport Channel Parameters:

Transport Channel:

Name:BCH
Identity:0

TTI (ms):20
EP Type:1/2 Rate Convolutional Coding
CRC Size:16
RM Attribute:1
First Interleave:On
Number Of Transport Formats:2

Transport Format Set:

Transport Format 0:

Number Of Transport Blocks:0
Transport Block Size In Bits:0

Transport Format 1:

Number Of Transport Blocks:1
Transport Block Size In Bits:246

RM Maximum Length:540

Transport Format Combination Set:

Number Of Transport Format Combinations:2

Transport Format Combinations 0:

Transport Format:0

Transport Format Combinations 1:

Transport Format:1

#### CPHY Transport Channel Configuration CNF

PHY LLA @ 00:01:14.760

BTS unit: 1:2
Channel No: 0 Name: P_CCPCH
CFN: 61

Message Details:

#### CMAC Configuration REQ

LLA MAC @ 00:01:14.780

BTS unit: 1:2
Channel No: 0 Name: P_CCPCH
CFN: 63

Message Details:

Configuration Parameters:

Number Of Transport Channels:1

Transport Channels:

Item Number 0:

Transport Channel Parameters:

Transport Channel:

Name:BCH
Identity:0

TTI (ms):20
EP Type:1/2 Rate Convolutional Coding
CRC Size:16
RM Attribute:1
First Interleave:On
Number Of Transport Formats:2

Transport Format Set:

Transport Format 0:

Number Of Transport Blocks:0
Transport Block Size In Bits:0

Transport Format 1:

Number Of Transport Blocks:1
Transport Block Size In Bits:246

Number Of Logical Channels:1

Logical Channels:

Item Number 0:

Logical Channel:

Name:BCCH
Identity:0

Priority:1
CT Length:0
CT Value:0
TCTF Length:0
TCTF Value:0
UE ID Type:Not used
UE ID:0

Active Flag:1

Transport Format Combination Set:

Number Of Transport Format Combinations:2

Transport Format Combinations 0:

Transport Format:0

Transport Format Combinations 1:

Transport Format:1

#### CMAC Configuration CNF

MAC LLA @ 00:01:14.780

BTS unit: 1:2
Channel No: 0 Name: P_CCPCH
CFN: 63

Message Details:

#### CMAC_Config_CNF

LLA RRC @ 00:01:14.790

Channel ID: P-CCPCH
Cell ID: 6

Message Details:

CMAC_Config_CNF:

cellId:6

routingInfo:

physicalChannelIdentity:4

#### CPHY_RL_Setup_REQ

RRC LLA @ 00:01:14.790

Channel ID: S-CCPCH#1
Cell ID: 6

Message Details:

CPHY_RL_Setup_REQ:

cellId:6

routingInfo:

physicalChannelIdentity:5

ratType:fdd

setupMessage: (CphyRlSetupReq)

physicalChannelInfo:

secondaryCCPCHInfo:

scramblingCode:0

dl_ChannelizationCode: (SF256_AndCodeNumber)

sf64:1

sCCPCHSlotFormat:8
timingOffset:0
positionFixedOrFlexible:flexible
sttd_Indicator:false
dl_TxPower:-2
powerOffsetOfTFCI_PO1:6
powerOffsetOfPILOT_PO3:6

#### CPHY Radio Link Setup REQ

LLA PHY @ 00:01:14.800

BTS unit: 1:2
Channel No: 0 Name: S_CCPCH
CFN: 65

Message Details:

Configuration Parameters:

Channel Offset:7680
Scrambling Code:2400
Symbol Rate:60k
Channelization Code:1
Adjust Time:0
Power in dBm:-50
Tx Diversity:Off
Slot Format:8
NumOfDpdch:1

#### CPHY Radio Link Setup CNF

PHY LLA @ 00:01:14.810

BTS unit: 1:2
Channel No: 0 Name: S_CCPCH
CFN: 66

Message Details:

#### CPHY_RL_Setup_CNF

LLA RRC @ 00:01:14.830

Channel ID: S-CCPCH#1
Cell ID: 6

Message Details:

CPHY_RL_Setup_CNF:

cellId:6

routingInfo:

physicalChannelIdentity:5

#### CPHY_TrCH_Config_REQ

RRC LLA @ 00:01:14.830

Channel ID: S-CCPCH#1
Cell ID: 6

Message Details:

CPHY_TrCH_Config_REQ:

cellId:6

routingInfo:

physicalChannelIdentity:5

ratType:fdd

trchConfigType:

nonDch:

configMessage: (CphyTrchConfigReq)

activationTime: (SS_ActivationTime)

activateNow:

ulconnectedTrCHList: Omit

ulTFCS: (TFCS) Omit

dlconnectedTrCHList:

:

trchid (TransportChannelIdentity):12
dl_TransportChannelType (SS_DL_TransportChannelType):pch

transportChannelInfo: (CommonOrDedicatedTFS)

tti:

tti10: (CommonOrDedicatedTF_InfoList)

CommonOrDedicatedTF_Info:

tb_Size:240

numberOfTbSizeList:

NumberOfTransportBlocks:

zero:

NumberOfTransportBlocks:

one:

logicalChannelList:

allSizes:

semistaticTF_Information:

channelCodingType:

convolutional (CodingRate):half

rateMatchingAttribute:230
crc_Size:crc16

:

trchid (TransportChannelIdentity):13
dl_TransportChannelType (SS_DL_TransportChannelType):fach

transportChannelInfo: (CommonOrDedicatedTFS)

tti:

tti10: (CommonOrDedicatedTF_InfoList)

CommonOrDedicatedTF_Info:

tb_Size:168

numberOfTbSizeList:

NumberOfTransportBlocks:

zero:

NumberOfTransportBlocks:

one:

NumberOfTransportBlocks:

small:2

logicalChannelList:

allSizes:

semistaticTF_Information:

channelCodingType:

convolutional (CodingRate):half

rateMatchingAttribute:220
crc_Size:crc16

:

trchid (TransportChannelIdentity):14
dl_TransportChannelType (SS_DL_TransportChannelType):fach

transportChannelInfo: (CommonOrDedicatedTFS)

tti:

tti10: (CommonOrDedicatedTF_InfoList)

CommonOrDedicatedTF_Info:

tb_Size:360

numberOfTbSizeList:

NumberOfTransportBlocks:

zero:

NumberOfTransportBlocks:

one:

logicalChannelList:

allSizes:

semistaticTF_Information:

channelCodingType:

turbo:

rateMatchingAttribute:130
crc_Size:crc16

dlTFCS: (TFCS)

normalTFCI_Signalling: (ExplicitTFCS_Configuration)

complete: (TFCS_ReconfAdd)

ctfcSize:

ctfc4Bit:

:

ctfc4:0

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:1

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:2

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:3

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:4

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:5

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:6

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:8

powerOffsetInformation:

gainFactorInformation:

signalledGainFactors:

modeSpecificInfo:

fdd:

gainFactorBetaC (GainFactor):11

gainFactorBetaD (GainFactor):15
referenceTFC_ID:0

powerOffsetPp_m: Omit

#### CPHY Transport Channel Configuration REQ

LLA PHY @ 00:01:14.840

BTS unit: 1:2
Channel No: 0 Name: S_CCPCH
CFN: 69

Message Details:

Configuration Parameters:

DTX Position:Flexible
Second Interleave:On
Puncture Limit:100
CCTrCH Length:1080
Number Of Transport Channels:3

Transport Channels:

Item Number 0:

Transport Channel Parameters:

Transport Channel:

Name:PCH
Identity:0

TTI (ms):10
EP Type:1/2 Rate Convolutional Coding
CRC Size:16
RM Attribute:230
First Interleave:On
Number Of Transport Formats:2

Transport Format Set:

Transport Format 0:

Number Of Transport Blocks:0
Transport Block Size In Bits:240

Transport Format 1:

Number Of Transport Blocks:1
Transport Block Size In Bits:240

RM Maximum Length:457

Item Number 1:

Transport Channel Parameters:

Transport Channel:

Name:FACH
Identity:0

TTI (ms):10
EP Type:1/2 Rate Convolutional Coding
CRC Size:16
RM Attribute:220
First Interleave:On
Number Of Transport Formats:3

Transport Format Set:

Transport Format 0:

Number Of Transport Blocks:0
Transport Block Size In Bits:168

Transport Format 1:

Number Of Transport Blocks:1
Transport Block Size In Bits:168

Transport Format 2:

Number Of Transport Blocks:2
Transport Block Size In Bits:168

RM Maximum Length:623

Item Number 2:

Transport Channel Parameters:

Transport Channel:

Name:FACH
Identity:1

TTI (ms):10
EP Type:Turbo Coding
CRC Size:16
RM Attribute:130
First Interleave:On
Number Of Transport Formats:2

Transport Format Set:

Transport Format 0:

Number Of Transport Blocks:0
Transport Block Size In Bits:360

Transport Format 1:

Number Of Transport Blocks:1
Transport Block Size In Bits:360

RM Maximum Length:558

Transport Format Combination Set:

Number Of Transport Format Combinations:8

Transport Format Combinations 0:

Transport Format:0
Transport Format:0
Transport Format:0

Transport Format Combinations 1:

Transport Format:1
Transport Format:0
Transport Format:0

Transport Format Combinations 2:

Transport Format:0
Transport Format:1
Transport Format:0

Transport Format Combinations 3:

Transport Format:1
Transport Format:1
Transport Format:0

Transport Format Combinations 4:

Transport Format:0
Transport Format:2
Transport Format:0

Transport Format Combinations 5:

Transport Format:1
Transport Format:2
Transport Format:0

Transport Format Combinations 6:

Transport Format:0
Transport Format:0
Transport Format:1

Transport Format Combinations 7:

Transport Format:0
Transport Format:1
Transport Format:1

#### CPHY Transport Channel Configuration CNF

PHY LLA @ 00:01:14.840

BTS unit: 1:2
Channel No: 0 Name: S_CCPCH
CFN: 69

Message Details:

#### CPHY_TrCH_Config_CNF

LLA RRC @ 00:01:14.870

Channel ID: S-CCPCH#1
Cell ID: 6

Message Details:

CPHY_TrCH_Config_CNF:

cellId:6

routingInfo:

physicalChannelIdentity:5

#### CMAC_Config_REQ

RRC LLA @ 00:01:14.870

Channel ID: S-CCPCH#1
Cell ID: 6

Message Details:

CMAC_Config_REQ:

cellId:6

routingInfo:

physicalChannelIdentity:5

ratType:fdd

configMessage:

setup: (CmacConfigReq)

activationTime: (SS_ActivationTime)

activateNow:

uE_Info:

u_RNTI: Omit

c_RNTI: Omit

trCHInfo:

ulconnectedTrCHList: Omit

ulTFCS: (TFCS) Omit

dlconnectedTrCHList:

:

trchid (TransportChannelIdentity):12

transportChannelInfo: (CommonOrDedicatedTFS)

tti:

tti10: (CommonOrDedicatedTF_InfoList)

CommonOrDedicatedTF_Info:

tb_Size:240

numberOfTbSizeList:

NumberOfTransportBlocks:

zero:

NumberOfTransportBlocks:

one:

logicalChannelList:

allSizes:

semistaticTF_Information:

channelCodingType:

convolutional (CodingRate):half

rateMatchingAttribute:230
crc_Size:crc16

:

trchid (TransportChannelIdentity):13

transportChannelInfo: (CommonOrDedicatedTFS)

tti:

tti10: (CommonOrDedicatedTF_InfoList)

CommonOrDedicatedTF_Info:

tb_Size:168

numberOfTbSizeList:

NumberOfTransportBlocks:

zero:

NumberOfTransportBlocks:

one:

NumberOfTransportBlocks:

small:2

logicalChannelList:

allSizes:

semistaticTF_Information:

channelCodingType:

convolutional (CodingRate):half

rateMatchingAttribute:220
crc_Size:crc16

:

trchid (TransportChannelIdentity):14

transportChannelInfo: (CommonOrDedicatedTFS)

tti:

tti10: (CommonOrDedicatedTF_InfoList)

CommonOrDedicatedTF_Info:

tb_Size:360

numberOfTbSizeList:

NumberOfTransportBlocks:

zero:

NumberOfTransportBlocks:

one:

logicalChannelList:

allSizes:

semistaticTF_Information:

channelCodingType:

turbo:

rateMatchingAttribute:130
crc_Size:crc16

dlTFCS: (TFCS)

normalTFCI_Signalling: (ExplicitTFCS_Configuration)

complete: (TFCS_ReconfAdd)

ctfcSize:

ctfc4Bit:

:

ctfc4:0

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:1

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:2

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:3

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:4

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:5

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:6

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:8

powerOffsetInformation:

gainFactorInformation:

signalledGainFactors:

modeSpecificInfo:

fdd:

gainFactorBetaC (GainFactor):11

gainFactorBetaD (GainFactor):15
referenceTFC_ID:0

powerOffsetPp_m: Omit

trCH_LogCHMapping: (TrCH_LogCHMappingList1)

ulconnectedTrCHList: Omit

dlconnectedTrCHList:

:

trchid (TransportChannelIdentity):12

trCH_LogCHMappingList:

TrCH_LogicalChannelMapping:

logicalChannel_Mapping:

dl_LogicalChannelMapping: (SS_DL_LogicalChannelMapping)

macHeaderManipulation (MAC_HeaderManipulation):normalMacHeader
dl_TransportChannelType (SS_DL_TransportChannelType):pch
logicalChannelIdentity:1
logicalChannelType:pCCH

rlc_SizeList:

configured:

mac_LogicalChannelPriority:1

rB_Identity:-2
cn_DomainIdentity: Omit

:

trchid (TransportChannelIdentity):13

trCH_LogCHMappingList:

TrCH_LogicalChannelMapping:

logicalChannel_Mapping:

dl_LogicalChannelMapping: (SS_DL_LogicalChannelMapping)

macHeaderManipulation (MAC_HeaderManipulation):normalMacHeader
dl_TransportChannelType (SS_DL_TransportChannelType):fach
logicalChannelIdentity:5
logicalChannelType:cCCH

rlc_SizeList:

configured:

mac_LogicalChannelPriority:1

rB_Identity:0
cn_DomainIdentity: Omit

#### CMAC_Config_CNF

LLA RRC @ 00:01:14.900

Channel ID: S-CCPCH#1
Cell ID: 6

Message Details:

CMAC_Config_CNF:

cellId:6

routingInfo:

physicalChannelIdentity:5

#### CPHY_RL_Setup_REQ

RRC LLA @ 00:01:14.900

Channel ID: PICH#1
Cell ID: 6

Message Details:

CPHY_RL_Setup_REQ:

cellId:6

routingInfo:

physicalChannelIdentity:6

ratType:fdd

setupMessage: (CphyRlSetupReq)

physicalChannelInfo:

pICHInfo:

pichinfo: (PICH_Info)

fdd:

channelisationCode256:2
pi_CountPerFrame:e18
sttd_Indicator:false

dl_TxPower (PICH_PowerOffset):-5
sccpchId_associated:5

#### CPHY Radio Link Setup REQ

LLA PHY @ 00:01:14.910

BTS unit: 1:2
Channel No: 0 Name: PICH
CFN: 76

Message Details:

Configuration Parameters:

Channel Offset:0
Scrambling Code:2400
Symbol Rate:15k
Channelization Code:2
Adjust Time:0
Power in dBm:-53
Tx Diversity:Off
NumOfDpdch:0
Np:18

#### CPHY Radio Link Setup CNF

PHY LLA @ 00:01:14.910

BTS unit: 1:2
Channel No: 0 Name: PICH
CFN: 76

Message Details:

#### CPHY_RL_Setup_CNF

LLA RRC @ 00:01:14.920

Channel ID: PICH#1
Cell ID: 6

Message Details:

CPHY_RL_Setup_CNF:

cellId:6

routingInfo:

physicalChannelIdentity:6

#### CPHY_RL_Setup_REQ

RRC LLA @ 00:01:14.920

Channel ID: AICH#1
Cell ID: 6

Message Details:

CPHY_RL_Setup_REQ:

cellId:6

routingInfo:

physicalChannelIdentity:7

ratType:fdd

setupMessage: (CphyRlSetupReq)

physicalChannelInfo:

aICHInfo:

aichinfo: (AICH_Info)

channelisationCode256:3
sttd_Indicator:false
aich_TransmissionTiming:e0

dl_TxPower (AICH_PowerOffset):-5

#### CPHY Radio Link Setup REQ

LLA PHY @ 00:01:14.930

BTS unit: 1:2
Channel No: 0 Name: AICH
CFN: 78

Message Details:

Configuration Parameters:

Channel Offset:7680
Scrambling Code:2400
Symbol Rate:15k
Channelization Code:3
Adjust Time:0
Power in dBm:-53
Tx Diversity:Off
AICH Transmission Timing:3 Access Slots
AICH Polarity:Positive
NumOfDpdch:0

#### CPHY Radio Link Setup CNF

PHY LLA @ 00:01:14.930

BTS unit: 1:2
Channel No: 0 Name: AICH
CFN: 78

Message Details:

#### CPHY_RL_Setup_CNF

LLA RRC @ 00:01:14.940

Channel ID: AICH#1
Cell ID: 6

Message Details:

CPHY_RL_Setup_CNF:

cellId:6

routingInfo:

physicalChannelIdentity:7

#### CPHY_RL_Setup_REQ

RRC LLA @ 00:01:14.940

Channel ID: PRACH#1
Cell ID: 6

Message Details:

CPHY_RL_Setup_REQ:

cellId:6

routingInfo:

physicalChannelIdentity:8

ratType:fdd

setupMessage: (CphyRlSetupReq)

physicalChannelInfo:

pRACHInfo:

fdd_tdd:

fdd:

preambleSignature (AvailableSignatures):0000000011111111
spreadingFactorForDataPart (SF_PRACH):sfpr64
preambleScramblingCode (PreambleScramblingCodeWordNumber):0
puncturingLimit:pl1
accessSlot (AvailableSubChannelNumbers):111111111111

#### CPHY_RL_Setup_CNF

LLA RRC @ 00:01:14.950

Channel ID: PRACH#1
Cell ID: 6

Message Details:

CPHY_RL_Setup_CNF:

cellId:6

routingInfo:

physicalChannelIdentity:8

#### CPHY_TrCH_Config_REQ

RRC LLA @ 00:01:14.950

Channel ID: PRACH#1
Cell ID: 6

Message Details:

CPHY_TrCH_Config_REQ:

cellId:6

routingInfo:

physicalChannelIdentity:8

ratType:fdd

trchConfigType:

nonDch:

configMessage: (CphyTrchConfigReq)

activationTime: (SS_ActivationTime)

activateNow:

ulconnectedTrCHList:

:

trchid (TransportChannelIdentity):15
ul_TransportChannelType (SS_UL_TransportChannelType):rach

transportChannelInfo: (CommonOrDedicatedTFS)

tti:

tti20: (CommonOrDedicatedTF_InfoList)

CommonOrDedicatedTF_Info:

tb_Size:168

numberOfTbSizeList:

NumberOfTransportBlocks:

one:

logicalChannelList:

configured:

CommonOrDedicatedTF_Info:

tb_Size:360

numberOfTbSizeList:

NumberOfTransportBlocks:

one:

logicalChannelList:

configured:

semistaticTF_Information:

channelCodingType:

convolutional (CodingRate):half

rateMatchingAttribute:150
crc_Size:crc16

ulTFCS: (TFCS)

normalTFCI_Signalling: (ExplicitTFCS_Configuration)

complete: (TFCS_ReconfAdd)

ctfcSize:

ctfc2Bit:

:

ctfc2:0

powerOffsetInformation: Omit

:

ctfc2:1

powerOffsetInformation: Omit

dlconnectedTrCHList: Omit

dlTFCS: (TFCS) Omit

#### CPHY Radio Link Setup REQ

LLA PHY @ 00:01:14.960

BTS unit: 1:2
Channel No: 0 Name: PRACH
CFN: 81

Message Details:

Configuration Parameters:

Channel Offset:10240
Scrambling Code:16779616
Symbol Rate:60k
Channelization Code:128
Adjust Time:0
Slot Format:2
NumOfDpdch:1

#### CPHY Radio Link Setup CNF

PHY LLA @ 00:01:14.960

BTS unit: 1:2
Channel No: 0 Name: PRACH
CFN: 81

Message Details:

#### CPHY Transport Channel Configuration REQ

LLA PHY @ 00:01:14.980

BTS unit: 1:2
Channel No: 0 Name: PRACH
CFN: 83

Message Details:

Configuration Parameters:

DTX Position:Flexible
Second Interleave:On
Puncture Limit:100
CCTrCH Length:600
Number Of Transport Channels:1

Transport Channels:

Item Number 0:

Transport Channel Parameters:

Transport Channel:

Name:RACH
Identity:0

TTI (ms):20
EP Type:1/2 Rate Convolutional Coding
CRC Size:16
RM Attribute:150
First Interleave:On
Number Of Transport Formats:2

Transport Format Set:

Transport Format 0:

Number Of Transport Blocks:1
Transport Block Size In Bits:168

Transport Format 1:

Number Of Transport Blocks:1
Transport Block Size In Bits:360

RM Maximum Length:600

Transport Format Combination Set:

Number Of Transport Format Combinations:2

Transport Format Combinations 0:

Transport Format:0

Transport Format Combinations 1:

Transport Format:1

#### PHY_DATA_REQ

MAC PHY @ 00:01:14.940

BTS unit: 2:1
Channel No: 0 Name: PCH
CFN: 79

Message Details:

TFI:1
TB set size:240
TB size:240
TB set (raw):

[0]21 00 00 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00 00 00 00 00
[24]00 00 00 00 00 00

TB set (decoded):

TB 0:

MAC SDU (240 bits):

[0]21 00 00 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00 00 00 00 00
[24]00 00 00 00 00 00

#### CPHY Transport Channel Configuration CNF

PHY LLA @ 00:01:14.990

BTS unit: 1:2
Channel No: 0 Name: PRACH
CFN: 84

Message Details:

#### CPHY_TrCH_Config_CNF

LLA RRC @ 00:01:15.000

Channel ID: PRACH#1
Cell ID: 6

Message Details:

CPHY_TrCH_Config_CNF:

cellId:6

routingInfo:

physicalChannelIdentity:8

#### CMAC_Config_REQ

RRC LLA @ 00:01:15.000

Channel ID: PRACH#1
Cell ID: 6

Message Details:

CMAC_Config_REQ:

cellId:6

routingInfo:

physicalChannelIdentity:8

ratType:fdd

configMessage:

setup: (CmacConfigReq)

activationTime: (SS_ActivationTime)

activateNow:

uE_Info:

u_RNTI: Omit

c_RNTI: Omit

trCHInfo:

ulconnectedTrCHList:

:

trchid (TransportChannelIdentity):15

transportChannelInfo: (CommonOrDedicatedTFS)

tti:

tti20: (CommonOrDedicatedTF_InfoList)

CommonOrDedicatedTF_Info:

tb_Size:168

numberOfTbSizeList:

NumberOfTransportBlocks:

one:

logicalChannelList:

configured:

CommonOrDedicatedTF_Info:

tb_Size:360

numberOfTbSizeList:

NumberOfTransportBlocks:

one:

logicalChannelList:

configured:

semistaticTF_Information:

channelCodingType:

convolutional (CodingRate):half

rateMatchingAttribute:150
crc_Size:crc16

ulTFCS: (TFCS)

normalTFCI_Signalling: (ExplicitTFCS_Configuration)

complete: (TFCS_ReconfAdd)

ctfcSize:

ctfc2Bit:

:

ctfc2:0

powerOffsetInformation: Omit

:

ctfc2:1

powerOffsetInformation: Omit

dlconnectedTrCHList: Omit

dlTFCS: (TFCS) Omit

trCH_LogCHMapping: (TrCH_LogCHMappingList1)

ulconnectedTrCHList:

:

trchid (TransportChannelIdentity):15

trCH_LogCHMappingList:

TrCH_LogicalChannelMapping:

logicalChannel_Mapping:

ul_LogicalChannelMapping: (SS_UL_LogicalChannelMapping)

macHeaderManipulation (MAC_HeaderManipulation):normalMacHeader
ul_TransportChannelType (SS_UL_TransportChannelType):rach
logicalChannelIdentity:5
logicalChannelType:cCCH

rB_Identity:0
cn_DomainIdentity: Omit

dlconnectedTrCHList: Omit

#### CMAC_Config_CNF

LLA RRC @ 00:01:15.010

Channel ID: PRACH#1
Cell ID: 6

Message Details:

CMAC_Config_CNF:

cellId:6

routingInfo:

physicalChannelIdentity:8

#### CRLC_Config_REQ

RRC LLA @ 00:01:15.010

Channel ID: RbBcch
Cell ID: 6

Message Details:

CRLC_Config_REQ:

cellId:6

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode) Omit

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):246

dl_RLCModeInfo: (UL_RLC_Mode)

ul_TM_RLC_Mode:

transmissionRLC_Discard: Omit

segmentationIndication:false

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity): Omit
dLlogicalChannelIdentity (LogicalChannelIdentity):1
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CMAC Configuration REQ

LLA MAC @ 00:01:15.010

BTS unit: 1:2
Channel No: 0 Name: PRACH
CFN: 86

Message Details:

Configuration Parameters:

Number Of Transport Channels:1

Transport Channels:

Item Number 0:

Transport Channel Parameters:

Transport Channel:

Name:RACH
Identity:0

TTI (ms):20
EP Type:1/2 Rate Convolutional Coding
CRC Size:16
RM Attribute:150
First Interleave:On
Number Of Transport Formats:2

Transport Format Set:

Transport Format 0:

Number Of Transport Blocks:1
Transport Block Size In Bits:168

Transport Format 1:

Number Of Transport Blocks:1
Transport Block Size In Bits:360

Number Of Logical Channels:1

Logical Channels:

Item Number 0:

Logical Channel:

Name:CCCH
Identity:0

Priority:0
CT Length:0
CT Value:0
TCTF Length:2
TCTF Value:0
UE ID Type:Not used
UE ID:0

Active Flag:1

Transport Format Combination Set:

Number Of Transport Format Combinations:2

Transport Format Combinations 0:

Transport Format:0

Transport Format Combinations 1:

Transport Format:1

#### CMAC Configuration CNF

MAC LLA @ 00:01:15.010

BTS unit: 1:2
Channel No: 0 Name: PRACH
CFN: 86

Message Details:

#### CRLC TM Channel Establish REQ

LLA RLC @ 00:01:15.020

BTS unit: 1:2
Channel No: 0 Name: BCCH
CFN: 87

Message Details:

Configuration Parameters:

Number Of PU Sizes:1

PU sizes In Bits:

Item 0:246

#### CRLC TM Channel Establish CNF

RLC LLA @ 00:01:15.020

BTS unit: 1:2
Channel No: 0 Name: BCCH
CFN: 87

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:01:15.030

Channel ID: RbBcch
Cell ID: 6

Message Details:

CRLC_Config_CNF:

cellId:6

routingInfo:

rB_Identity:-1

#### CRLC_Config_REQ

RRC LLA @ 00:01:15.140

Channel ID: RbPcch
Cell ID: 6

Message Details:

CRLC_Config_REQ:

cellId:6

routingInfo:

rB_Identity:-2

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode) Omit

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):240

dl_RLCModeInfo: (UL_RLC_Mode)

ul_TM_RLC_Mode:

transmissionRLC_Discard: Omit

segmentationIndication:false

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity): Omit
dLlogicalChannelIdentity (LogicalChannelIdentity):1
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC_Config_CNF

LLA RRC @ 00:01:15.150

Channel ID: RbPcch
Cell ID: 6

Message Details:

CRLC_Config_CNF:

cellId:6

routingInfo:

rB_Identity:-2

#### CRLC_Config_REQ

RRC LLA @ 00:01:15.150

Channel ID: Rb0
Cell ID: 6

Message Details:

CRLC_Config_REQ:

cellId:6

routingInfo:

rB_Identity:0

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode) Omit

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):152

dl_RLCModeInfo: (UL_RLC_Mode)

ul_UM_RLC_Mode:

transmissionRLC_Discard:

timerBasedNoExplicit (NoExplicitDiscard):dt100

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity): Omit
dLlogicalChannelIdentity (LogicalChannelIdentity):5
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC TM Channel Establish REQ

LLA RLC @ 00:01:15.150

BTS unit: 1:2
Channel No: 0 Name: PCCH
CFN: 100

Message Details:

Configuration Parameters:

Number Of PU Sizes:1

PU sizes In Bits:

Item 0:240

#### CRLC TM Channel Establish CNF

RLC LLA @ 00:01:15.150

BTS unit: 1:2
Channel No: 0 Name: PCCH
CFN: 100

Message Details:

#### CRLC UM Channel Establish REQ

LLA RLC @ 00:01:15.160

BTS unit: 1:2
Channel No: 1 Name: CCCH
CFN: 101

Message Details:

Configuration Parameters:

PU Size In Bits:152

#### CRLC UM Channel Establish CNF

RLC LLA @ 00:01:15.160

BTS unit: 1:2
Channel No: 1 Name: CCCH
CFN: 101

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:01:15.170

Channel ID: Rb0
Cell ID: 6

Message Details:

CRLC_Config_CNF:

cellId:6

routingInfo:

rB_Identity:0

#### CRLC_Config_REQ

RRC LLA @ 00:01:15.170

Channel ID: Rb0
Cell ID: 6

Message Details:

CRLC_Config_REQ:

cellId:6

routingInfo:

rB_Identity:0

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode)

dl_TM_RLC_Mode:

segmentationIndication:false

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):166

dl_RLCModeInfo: (UL_RLC_Mode)

ul_TM_RLC_Mode:

transmissionRLC_Discard: Omit

segmentationIndication:false

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity):5
dLlogicalChannelIdentity (LogicalChannelIdentity): Omit
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC TM Channel Establish REQ

LLA RLC @ 00:01:15.180

BTS unit: 1:2
Channel No: 0 Name: CCCH
CFN: 103

Message Details:

Configuration Parameters:

Number Of PU Sizes:1

PU sizes In Bits:

Item 0:166

#### CRLC TM Channel Establish CNF

RLC LLA @ 00:01:15.180

BTS unit: 1:2
Channel No: 0 Name: CCCH
CFN: 103

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:01:15.190

Channel ID: Rb0
Cell ID: 6

Message Details:

CRLC_Config_CNF:

cellId:6

routingInfo:

rB_Identity:0

#### o_SIB_PER_Encoding

RRC RRC @ 00:01:15.200

Category: TSO

Message Details:

Inputs:

SIB:

sIB1: (SysInfoType1)

cn_CommonGSM_MAP_NAS_SysInfo (NAS_SystemInformationGSM_MAP):

[0]00 01

cn_DomainSysInfoList:

CN_DomainSysInfo:

cn_DomainIdentity:ps_domain

cn_Type:

gsm_MAP (NAS_SystemInformationGSM_MAP):

[0]01 00

cn_DRX_CycleLengthCoeff (CN_DRX_CycleLengthCoefficient):7

CN_DomainSysInfo:

cn_DomainIdentity:cs_domain

cn_Type:

gsm_MAP (NAS_SystemInformationGSM_MAP):

[0]1E 01

cn_DRX_CycleLengthCoeff (CN_DRX_CycleLengthCoefficient):7

ue_ConnTimersAndConstants:

t_301:ms2000
n_301:2
t_302:ms4000
n_302:3
t_304:ms1000
n_304:3
t_305:m60
t_307:s50
t_308:ms320
t_309:8
t_310:ms320
n_310:5
t_311:ms500
t_312:5
n_312:s200
t_313:10
n_313:s20
t_314:s20
t_315:s30
n_315:s200
t_316:s50
t_317:s1800

ue_IdleTimersAndConstants:

t_300:ms4000
n_300:7
t_312:10
n_312:s200

v3a0NonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]11 00 01 00 00 00 00 00
[8]00 00 01 01 10 00 10 00
[16]00 00 10 00 00 00 00 10
[24]00 01 00 01 11 10 00 00
[32]00 01 01 00 00 11 11 11
[40]11 11 11 01 11 11 01 10
[48]11 10 01 10 11 11 11 11
[56]10 10 01 01 01 01 11 01
[64]01 11 01 00 11 10 11 11
[72]11 00 11 11 01 00 11

#### o_SIB_PER_Encoding

RRC RRC @ 00:01:15.200

Category: TSO

Message Details:

Inputs:

SIB:

sIB2: (SysInfoType2)

ura_IdentityList:

URA_Identity:0000000000000100

nonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]00 00 00 00 00 00 00 00
[8]01 00

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:01:15.200

Channel ID: RbBcch
Cell ID: 6

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:6

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:10
bcch_ModificationTime: Omit

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:01:15.220

Channel ID: RbBcch
Cell ID: 6

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:6

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:01:15.220

Channel ID: RbBcch
Cell ID: 6

Message Details:

RLC_TR_DATA_REQ:

cellId:6

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

completeSIB_List:

CompleteSIBshort:

sib_Type:systemInformationBlockType1
sib_Data_variable:11000100000000000000010110001000000010000000001000010001111000000001010000111111111111011111011011100110111111111010010101011101011101001110111111001111010011

CompleteSIBshort:

sib_Type:systemInformationBlockType2
sib_Data_variable:00000000000000000100

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:01:15.220

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 20

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

completeSIB_List:

CompleteSIB_List.element:

sib_Type: systemInformationBlockType1_SIB_Type [enum=1]

sib_Data_variable: 11000100000000000000010110001000000010000000001000010001111000000001010000111111111111011111011011100110111111111010010101011101011101001110111111001111010011

CompleteSIB_List.element:

sib_Type: systemInformationBlockType2_SIB_Type [enum=2]

sib_Data_variable: 00000000000000000100

Layer 3 SDU:

[0]00 0E 21 9D C4 00 05 88
[8]08 02 11 E0 14 3F FD F6
[16]E6 FF A5 5D 74 EF CF 4C
[24]42 60 00 08

#### o_SIB_PER_Encoding

RRC RRC @ 00:01:15.220

Category: TSO

Message Details:

Inputs:

SIB:

sIB2: (SysInfoType2)

ura_IdentityList:

URA_Identity:0000000000000100

nonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]00 00 00 00 00 00 00 00
[8]01 00

#### o_SIB_PER_Encoding

RRC RRC @ 00:01:15.230

Category: TSO

Message Details:

Inputs:

SIB:

sIB1: (SysInfoType1)

cn_CommonGSM_MAP_NAS_SysInfo (NAS_SystemInformationGSM_MAP):

[0]00 01

cn_DomainSysInfoList:

CN_DomainSysInfo:

cn_DomainIdentity:ps_domain

cn_Type:

gsm_MAP (NAS_SystemInformationGSM_MAP):

[0]01 00

cn_DRX_CycleLengthCoeff (CN_DRX_CycleLengthCoefficient):7

CN_DomainSysInfo:

cn_DomainIdentity:cs_domain

cn_Type:

gsm_MAP (NAS_SystemInformationGSM_MAP):

[0]1E 01

cn_DRX_CycleLengthCoeff (CN_DRX_CycleLengthCoefficient):7

ue_ConnTimersAndConstants:

t_301:ms2000
n_301:2
t_302:ms4000
n_302:3
t_304:ms1000
n_304:3
t_305:m60
t_307:s50
t_308:ms320
t_309:8
t_310:ms320
n_310:5
t_311:ms500
t_312:5
n_312:s200
t_313:10
n_313:s20
t_314:s20
t_315:s30
n_315:s200
t_316:s50
t_317:s1800

ue_IdleTimersAndConstants:

t_300:ms4000
n_300:7
t_312:10
n_312:s200

v3a0NonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]11 00 01 00 00 00 00 00
[8]00 00 01 01 10 00 10 00
[16]00 00 10 00 00 00 00 10
[24]00 01 00 01 11 10 00 00
[32]00 01 01 00 00 11 11 11
[40]11 11 11 01 11 11 01 10
[48]11 10 01 10 11 11 11 11
[56]10 10 01 01 01 01 11 01
[64]01 11 01 00 11 10 11 11
[72]11 00 11 11 01 00 11

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:01:15.230

Channel ID: RbBcch
Cell ID: 6

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:6

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:10
bcch_ModificationTime: Omit

#### MAC_DATA_REQ

RLC MAC @ 00:01:15.240

Category: Configuration
BTS unit: 1:2
Channel No: 0 Name: BCCH
CFN: 109

Message Details:

RLC PDU size (bits):224
RLC PDU (raw):

[0]00 0E 21 9D C4 00 05 88
[8]08 02 11 E0 14 3F FD F6
[16]E6 FF A5 5D 74 EF CF 4C
[24]42 60 00 08

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:01:15.250

Channel ID: RbBcch
Cell ID: 6

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:6

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:01:15.250

Channel ID: RbBcch
Cell ID: 6

Message Details:

RLC_TR_DATA_REQ:

cellId:6

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

completeSIB_List:

CompleteSIBshort:

sib_Type:systemInformationBlockType1
sib_Data_variable:11000100000000000000010110001000000010000000001000010001111000000001010000111111111111011111011011100110111111111010010101011101011101001110111111001111010011

CompleteSIBshort:

sib_Type:systemInformationBlockType2
sib_Data_variable:00000000000000000100

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:01:15.250

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 20

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

completeSIB_List:

CompleteSIB_List.element:

sib_Type: systemInformationBlockType1_SIB_Type [enum=1]

sib_Data_variable: 11000100000000000000010110001000000010000000001000010001111000000001010000111111111111011111011011100110111111111010010101011101011101001110111111001111010011

CompleteSIB_List.element:

sib_Type: systemInformationBlockType2_SIB_Type [enum=2]

sib_Data_variable: 00000000000000000100

Layer 3 SDU:

[0]00 0E 21 9D C4 00 05 88
[8]08 02 11 E0 14 3F FD F6
[16]E6 FF A5 5D 74 EF CF 4C
[24]42 60 00 08

#### o_SIB_PER_Encoding

RRC RRC @ 00:01:15.250

Category: TSO

Message Details:

Inputs:

SIB:

sIB3: (SysInfoType3)

sib4indicator:true
cellIdentity:0000000000000000000000000110

cellSelectReselectInfo: (CellSelectReselectInfoSIB_3_4)

mappingInfo: Omit

cellSelectQualityMeasure:

cpich_RSCP:

modeSpecificInfo:

fdd:

s_Intrasearch (S_SearchQual):8
s_Intersearch (S_SearchQual):8
s_SearchHCS (S_SearchRXLEV): Omit

rat_List: (RAT_FDD_InfoList)

RAT_FDD_Info:

rat_Identifier:gsm
s_SearchRAT (S_SearchQual):-16
s_HCS_RAT (S_SearchRXLEV): Omit
s_Limit_SearchRAT (S_SearchQual):0

q_QualMin:-24
q_RxlevMin:-40

q_Hyst_l_S (Q_Hyst_S):2
t_Reselection_S:0

hcs_ServingCellInformation: Omit

maxAllowedUL_TX_Power:21

cellAccessRestriction:

cellBarred:

notBarred:

cellReservedForOperatorUse (ReservedIndicator):notReserved
cellReservationExtension (ReservedIndicator):notReserved

accessClassBarredList:

AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred

nonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]01 00 00 00 00 00 00 00
[8]00 00 00 00 00 01 10 00
[16]10 11 01 11 00 01 10 00
[24]00 00 00 00 00 01 00 00
[32]00 00 00 10 01 00 00 10
[40]00 00 01 00 01 11 11 11
[48]11 11 11 11 11 11 11 11

#### o_SIB_PER_Encoding

RRC RRC @ 00:01:15.250

Category: TSO

Message Details:

Inputs:

SIB:

sIB7: (SysInfoType7)

modeSpecificInfo:

fdd:

ul_Interference:-100

prach_Information_SIB5_List: (DynamicPersistenceLevelList)

DynamicPersistenceLevel:2

prach_Information_SIB6_List: (DynamicPersistenceLevelList)

DynamicPersistenceLevel:2

expirationTimeFactor: Omit

nonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]10 00 00 10 10 00 00 00
[8]10 00 00 01

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:01:15.250

Channel ID: RbBcch
Cell ID: 6

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:6

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:7
bcch_ModificationTime: Omit

#### PHY_DATA_REQ

MAC PHY @ 00:01:15.250

BTS unit: 1:2
Channel No: 0 Name: BCH
CFN: 110

Message Details:

SIB repetition period:64
SIB position:20
SIB size:246
SIB (raw):

[0]00 0E 21 9D C4 00 05 88
[8]08 02 11 E0 14 3F FD F6
[16]E6 FF A5 5D 74 EF CF 4C
[24]42 60 00 08 10 C2 50 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 0E 21 9D C4 00 05 88
[8]08 02 11 E0 14 3F FD F6
[16]E6 FF A5 5D 74 EF CF 4C
[24]42 60 00 08 10 C2 50

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:01:15.260

Channel ID: RbBcch
Cell ID: 6

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:6

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:01:15.260

Channel ID: RbBcch
Cell ID: 6

Message Details:

RLC_TR_DATA_REQ:

cellId:6

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

completeSIB_List:

CompleteSIBshort:

sib_Type:systemInformationBlockType7
sib_Data_variable:100000101000000010000001

CompleteSIBshort:

sib_Type:systemInformationBlockType3
sib_Data_variable:0100000000000000000000000001100010110111000110000000000000010000000000100100001000000100011111111111111111111111

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:01:15.260

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 14

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

completeSIB_List:

CompleteSIB_List.element:

sib_Type: systemInformationBlockType7_SIB_Type [enum=7]

sib_Data_variable: 100000101000000010000001

CompleteSIB_List.element:

sib_Type: systemInformationBlockType3_SIB_Type [enum=3]

sib_Data_variable: 0100000000000000000000000001100010110111000110000000000000010000000000100100001000000100011111111111111111111111

Layer 3 SDU:

[0]00 0E 27 17 82 80 81 1B
[8]7A 00 00 00 C5 B8 C0 00
[16]80 12 10 23 FF FF F8

#### o_SIB_PER_Encoding

RRC RRC @ 00:01:15.260

Category: TSO

Message Details:

Inputs:

SIB:

sIB4: (SysInfoType4)

cellIdentity:0000000000000000000000000110

cellSelectReselectInfo: (CellSelectReselectInfoSIB_3_4)

mappingInfo: Omit

cellSelectQualityMeasure:

cpich_RSCP:

modeSpecificInfo:

fdd:

s_Intrasearch (S_SearchQual):8
s_Intersearch (S_SearchQual):8
s_SearchHCS (S_SearchRXLEV): Omit

rat_List: (RAT_FDD_InfoList)

RAT_FDD_Info:

rat_Identifier:gsm
s_SearchRAT (S_SearchQual):-16
s_HCS_RAT (S_SearchRXLEV): Omit
s_Limit_SearchRAT (S_SearchQual):0

q_QualMin:-24
q_RxlevMin:-40

q_Hyst_l_S (Q_Hyst_S):0
t_Reselection_S:0

hcs_ServingCellInformation: Omit

maxAllowedUL_TX_Power:21

cellAccessRestriction:

cellBarred:

notBarred:

cellReservedForOperatorUse (ReservedIndicator):notReserved
cellReservationExtension (ReservedIndicator):notReserved

accessClassBarredList: Omit

nonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]00 00 00 00 00 00 00 00
[8]00 00 00 00 00 11 00 01
[16]01 10 11 10 00 11 00 00
[24]00 00 00 00 00 10 00 00
[32]00 00 01 00 10 00 00 00
[40]00 00 10 00 11 10 11 1

#### MAC_DATA_REQ

RLC MAC @ 00:01:15.270

Category: Configuration
BTS unit: 1:2
Channel No: 0 Name: BCCH
CFN: 112

Message Details:

RLC PDU size (bits):224
RLC PDU (raw):

[0]00 0E 21 9D C4 00 05 88
[8]08 02 11 E0 14 3F FD F6
[16]E6 FF A5 5D 74 EF CF 4C
[24]42 60 00 08

#### MAC_DATA_REQ

RLC MAC @ 00:01:15.270

Category: Configuration
BTS unit: 1:2
Channel No: 0 Name: BCCH
CFN: 112

Message Details:

RLC PDU size (bits):184
RLC PDU (raw):

[0]00 0E 27 17 82 80 81 1B
[8]7A 00 00 00 C5 B8 C0 00
[16]80 12 10 23 FF FF F8

#### PHY_DATA_REQ

MAC PHY @ 00:01:15.270

BTS unit: 1:2
Channel No: 0 Name: BCH
CFN: 112

Message Details:

SIB repetition period:64
SIB position:20
SIB size:246
SIB (raw):

[0]00 0E 21 9D C4 00 05 88
[8]08 02 11 E0 14 3F FD F6
[16]E6 FF A5 5D 74 EF CF 4C
[24]42 60 00 08 10 C2 50 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 0E 21 9D C4 00 05 88
[8]08 02 11 E0 14 3F FD F6
[16]E6 FF A5 5D 74 EF CF 4C
[24]42 60 00 08 10 C2 50

#### o_SIB_PER_Encoding

RRC RRC @ 00:01:15.280

Category: TSO

Message Details:

Inputs:

SIB:

sIB7: (SysInfoType7)

modeSpecificInfo:

fdd:

ul_Interference:-100

prach_Information_SIB5_List: (DynamicPersistenceLevelList)

DynamicPersistenceLevel:2

prach_Information_SIB6_List: (DynamicPersistenceLevelList)

DynamicPersistenceLevel:2

expirationTimeFactor: Omit

nonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]10 00 00 10 10 00 00 00
[8]10 00 00 01

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:01:15.280

Channel ID: RbBcch
Cell ID: 6

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:6

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:31
bcch_ModificationTime: Omit

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:01:15.290

Channel ID: RbBcch
Cell ID: 6

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:6

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:01:15.290

Channel ID: RbBcch
Cell ID: 6

Message Details:

RLC_TR_DATA_REQ:

cellId:6

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

completeSIB_List:

CompleteSIBshort:

sib_Type:systemInformationBlockType7
sib_Data_variable:100000101000000010000001

CompleteSIBshort:

sib_Type:systemInformationBlockType4
sib_Data_variable:00000000000000000000000000110001011011100011000000000000001000000000010010000000000010001110111

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:01:15.290

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 62

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

completeSIB_List:

CompleteSIB_List.element:

sib_Type: systemInformationBlockType7_SIB_Type [enum=7]

sib_Data_variable: 100000101000000010000001

CompleteSIB_List.element:

sib_Type: systemInformationBlockType4_SIB_Type [enum=4]

sib_Data_variable: 00000000000000000000000000110001011011100011000000000000001000000000010010000000000010001110111

Layer 3 SDU:

[0]00 0E 27 17 82 80 81 22
[8]F0 00 00 01 8B 71 80 01
[16]00 24 00 47 70

#### PHY_DATA_REQ

MAC PHY @ 00:01:15.290

BTS unit: 1:2
Channel No: 0 Name: BCH
CFN: 114

Message Details:

SIB repetition period:64
SIB position:14
SIB size:246
SIB (raw):

[0]00 0E 27 17 82 80 81 1B
[8]7A 00 00 00 C5 B8 C0 00
[16]80 12 10 23 FF FF F8 4C
[24]42 60 00 08 10 C2 50 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 0E 27 17 82 80 81 1B
[8]7A 00 00 00 C5 B8 C0 00
[16]80 12 10 23 FF FF F8 4C
[24]42 60 00 08 10 C2 50

#### o_SIB_PER_Encoding

RRC RRC @ 00:01:15.310

Category: TSO

Message Details:

Inputs:

SIB:

sIB5: (SysInfoType5)

sib6indicator:true
pich_PowerOffset:-5

modeSpecificInfo:

fdd:

aich_PowerOffset:-5

primaryCCPCH_Info: Omit

prach_SystemInformationList:

PRACH_SystemInformation:

prach_RACH_Info:

modeSpecificInfo:

fdd:

availableSignatures:0000000011111111
availableSF (SF_PRACH):sfpr64
preambleScramblingCodeWordNumber:0
puncturingLimit:pl1
availableSubChannelNumbers:111111111111

transportChannelIdentity:15

rach_TransportFormatSet: (TransportFormatSet)

commonTransChTFS:

tti:

tti20: (CommonDynamicTF_InfoList)

CommonDynamicTF_Info:

rlc_Size:

fdd:

octetModeRLC_SizeInfoType2:

sizeType1:15

numberOfTbSizeList:

NumberOfTransportBlocks:

one:

logicalChannelList:

configured:

CommonDynamicTF_Info:

rlc_Size:

fdd:

octetModeRLC_SizeInfoType2:

sizeType2:3

numberOfTbSizeList:

NumberOfTransportBlocks:

one:

logicalChannelList:

configured:

semistaticTF_Information:

channelCodingType:

convolutional (CodingRate):half

rateMatchingAttribute:150
crc_Size:crc16

rach_TFCS: (TFCS)

normalTFCI_Signalling: (ExplicitTFCS_Configuration)

complete: (TFCS_ReconfAdd)

ctfcSize:

ctfc2Bit:

:

ctfc2:0

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m:0

:

ctfc2:1

powerOffsetInformation:

gainFactorInformation:

signalledGainFactors:

modeSpecificInfo:

fdd:

gainFactorBetaC (GainFactor):11

gainFactorBetaD (GainFactor):15
referenceTFC_ID:0

powerOffsetPp_m:0

prach_Partitioning:

fdd:

ASCSetting_FDD:

accessServiceClass_FDD: Omit

ASCSetting_FDD:

accessServiceClass_FDD:

availableSignatureStartIndex:0
availableSignatureEndIndex:7
assignedSubChannelNumber:1111

ASCSetting_FDD:

accessServiceClass_FDD: Omit

ASCSetting_FDD:

accessServiceClass_FDD:

availableSignatureStartIndex:0
availableSignatureEndIndex:7
assignedSubChannelNumber:1111

ASCSetting_FDD:

accessServiceClass_FDD: Omit

ASCSetting_FDD:

accessServiceClass_FDD:

availableSignatureStartIndex:0
availableSignatureEndIndex:7
assignedSubChannelNumber:1111

ASCSetting_FDD:

accessServiceClass_FDD: Omit

ASCSetting_FDD:

accessServiceClass_FDD:

availableSignatureStartIndex:0
availableSignatureEndIndex:7
assignedSubChannelNumber:1111

persistenceScalingFactorList:

PersistenceScalingFactor:psf0_9
PersistenceScalingFactor:psf0_9
PersistenceScalingFactor:psf0_9
PersistenceScalingFactor:psf0_9
PersistenceScalingFactor:psf0_9
PersistenceScalingFactor:psf0_9

ac_To_ASC_MappingTable:

AC_To_ASC_Mapping:6
AC_To_ASC_Mapping:5
AC_To_ASC_Mapping:4
AC_To_ASC_Mapping:3
AC_To_ASC_Mapping:2
AC_To_ASC_Mapping:1
AC_To_ASC_Mapping:0

modeSpecificInfo:

fdd:

primaryCPICH_TX_Power:31
constantValue:-10

prach_PowerOffset:

powerRampStep:3
preambleRetransMax:4

rach_TransmissionParameters:

mmax:2
nb01Min (NB01):3
nb01Max (NB01):10

aich_Info:

channelisationCode256:3
sttd_Indicator:false
aich_TransmissionTiming:e0

sCCPCH_SystemInformationList:

SCCPCH_SystemInformation:

secondaryCCPCH_Info:

modeSpecificInfo:

fdd:

dummy1 (PCPICH_UsageForChannelEst):mayBeUsed

dummy2: (SecondaryCPICH_Info) Omit

secondaryScramblingCode: Omit
sttd_Indicator:false

sf_AndCodeNumber: (SF256_AndCodeNumber)

sf64:1

pilotSymbolExistence:false
tfci_Existence:true
positionFixedOrFlexible:flexible
timingOffset:0

tfcs:

normalTFCI_Signalling: (ExplicitTFCS_Configuration)

complete: (TFCS_ReconfAdd)

ctfcSize:

ctfc4Bit:

:

ctfc4:0

powerOffsetInformation: Omit

:

ctfc4:1

powerOffsetInformation: Omit

:

ctfc4:2

powerOffsetInformation: Omit

:

ctfc4:3

powerOffsetInformation: Omit

:

ctfc4:4

powerOffsetInformation: Omit

:

ctfc4:5

powerOffsetInformation: Omit

:

ctfc4:6

powerOffsetInformation: Omit

:

ctfc4:8

powerOffsetInformation: Omit

fach_PCH_InformationList:

FACH_PCH_Information:

transportFormatSet:

commonTransChTFS:

tti:

tti10: (CommonDynamicTF_InfoList)

CommonDynamicTF_Info:

rlc_Size:

fdd:

octetModeRLC_SizeInfoType2:

sizeType1:24

numberOfTbSizeList:

NumberOfTransportBlocks:

zero:

NumberOfTransportBlocks:

one:

logicalChannelList:

allSizes:

semistaticTF_Information:

channelCodingType:

convolutional (CodingRate):half

rateMatchingAttribute:230
crc_Size:crc16

transportChannelIdentity:12
ctch_Indicator:false

FACH_PCH_Information:

transportFormatSet:

commonTransChTFS:

tti:

tti10: (CommonDynamicTF_InfoList)

CommonDynamicTF_Info:

rlc_Size:

fdd:

octetModeRLC_SizeInfoType2:

sizeType1:15

numberOfTbSizeList:

NumberOfTransportBlocks:

zero:

NumberOfTransportBlocks:

one:

NumberOfTransportBlocks:

small:2

logicalChannelList:

allSizes:

semistaticTF_Information:

channelCodingType:

convolutional (CodingRate):half

rateMatchingAttribute:220
crc_Size:crc16

transportChannelIdentity:13
ctch_Indicator:false

FACH_PCH_Information:

transportFormatSet:

commonTransChTFS:

tti:

tti10: (CommonDynamicTF_InfoList)

CommonDynamicTF_Info:

rlc_Size:

fdd:

octetModeRLC_SizeInfoType2:

sizeType2:3

numberOfTbSizeList:

NumberOfTransportBlocks:

zero:

NumberOfTransportBlocks:

one:

logicalChannelList:

allSizes:

semistaticTF_Information:

channelCodingType:

turbo:

rateMatchingAttribute:130
crc_Size:crc16

transportChannelIdentity:14
ctch_Indicator:false

pich_Info:

fdd:

channelisationCode256:2
pi_CountPerFrame:e18
sttd_Indicator:false

cbs_DRX_Level1Information: Omit

nonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]00 01 01 01 01 00 01 00
[8]00 11 11 10 00 00 00 00
[16]11 11 11 11 01 00 00 11
[24]11 11 11 11 11 11 11 01
[32]11 01 00 10 00 01 00 00
[40]11 11 00 00 00 10 10 01
[48]00 00 11 00 00 00 10 10
[56]10 10 01 01 01 01 10 00
[64]00 00 00 00 00 00 11 00
[72]11 00 01 01 10 11 01 01
[80]01 11 11 10 00 10 10 11
[88]10 10 00 00 11 11 11 10
[96]10 00 00 11 11 11 10 10
[104]00 00 11 11 11 10 10 00
[112]00 11 11 11 11 01 00 00
[120]00 00 00 00 00 00 00 11
[128]01 01 10 00 11 01 00 01
[136]00 00 11 11 11 01 00 11
[144]10 01 01 00 00 01 10 00
[152]01 00 00 11 00 10 10 00
[160]00 00 11 00 00 00 11 10
[168]00 00 01 00 00 00 01 01
[176]10 00 00 10 00 00 00 11
[184]10 00 00 00 00 10 00 10
[192]00 01 10 01 00 00 10 10
[200]01 10 01 00 00 10 10 00
[208]00 00 00 00 11 00 00 00
[216]01 00 01 00 01 01 11 00
[224]10 10 11 01 01 10 10 00
[232]00 00 00 00 01 11 10 00
[240]10 00 01 10 00 00 00 01
[248]01 10 11 01 10 11 01 10
[256]00 10 00 00 00 00 01 00
[264]00 11 00 00 10 00 10 01
[272]01 00 00 00 10 11 01 10
[280]10 00 00 00 01 00 00

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:01:15.330

Channel ID: RbBcch
Cell ID: 6

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:6

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:22
bcch_ModificationTime: Omit

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:01:15.340

Channel ID: RbBcch
Cell ID: 6

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:6

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:01:15.340

Channel ID: RbBcch
Cell ID: 6

Message Details:

RLC_TR_DATA_REQ:

cellId:6

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

noSegment:

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:01:15.340

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 44

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

noSegment: NULL

Layer 3 SDU:

[0]00 00

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:01:15.340

Channel ID: RbBcch
Cell ID: 6

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:6

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:18
bcch_ModificationTime: Omit

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:01:15.360

Channel ID: RbBcch
Cell ID: 6

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:6

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:01:15.360

Channel ID: RbBcch
Cell ID: 6

Message Details:

RLC_TR_DATA_REQ:

cellId:6

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

firstSegment:

sib_Type:systemInformationBlockType5
seg_Count (SegCount):3
sib_Data_fixed:000101010100010000111110000000001111111101000011111111111111110111010010000100001111000000101001000011000000101010100101010110000000000000001100110001011011010101111110001010111010000011111110100000111111101000001111111010

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:01:15.360

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 36

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

firstSegment:

sib_Type: systemInformationBlockType5_SIB_Type [enum=5]

seg_Count: 3

sib_Data_fixed: 000101010100010000111110000000001111111101000011111111111111110111010010000100001111000000101001000011000000101010100101010110000000000000001100110001011011010101111110001010111010000011111110100000111111101000001111111010

Layer 3 SDU:

[0]00 02 52 15 44 3E 00 FF
[8]43 FF FD D2 10 F0 29 0C
[16]0A A5 58 00 0C C5 B5 7E
[24]2B A0 FE 83 FA 0F E8

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:01:15.360

Channel ID: RbBcch
Cell ID: 6

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:6

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:19
bcch_ModificationTime: Omit

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:01:15.370

Channel ID: RbBcch
Cell ID: 6

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:6

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:01:15.370

Channel ID: RbBcch
Cell ID: 6

Message Details:

RLC_TR_DATA_REQ:

cellId:6

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

subsequentSegment:

sib_Type:systemInformationBlockType5
segmentIndex:1
sib_Data_fixed:000011111111010000000000000000001101011000110100010000111111010011100101000001100001000011001010000000110000001110000001000000010110000010000000111000000000100010000110010000101001100100001010000000000011000000010001000101

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:01:15.370

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 38

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

subsequentSegment:

sib_Type: systemInformationBlockType5_SIB_Type [enum=5]

segmentIndex: 1

sib_Data_fixed: 000011111111010000000000000000001101011000110100010000111111010011100101000001100001000011001010000000110000001110000001000000010110000010000000111000000000100010000110010000101001100100001010000000000011000000010001000101

Layer 3 SDU:

[0]00 04 50 0F F4 00 00 D6
[8]34 43 F4 E5 06 10 CA 03
[16]03 81 01 60 80 E0 08 86
[24]42 99 0A 00 30 11 14

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:01:15.370

Channel ID: RbBcch
Cell ID: 6

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:6

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:21
bcch_ModificationTime: Omit

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:01:15.390

Channel ID: RbBcch
Cell ID: 6

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:6

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:01:15.390

Channel ID: RbBcch
Cell ID: 6

Message Details:

RLC_TR_DATA_REQ:

cellId:6

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

lastSegmentShort:

sib_Type:systemInformationBlockType5
segmentIndex:2
sib_Data_variable:1100101011010110100000000000011110001000011000000001011011011011011000100000000001000011000010001001010000001011011010000000010000

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:01:15.390

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 42

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

lastSegmentShort:

sib_Type: systemInformationBlockType5_SIB_Type [enum=5]

segmentIndex: 2

sib_Data_variable: 1100101011010110100000000000011110001000011000000001011011011011011000100000000001000011000010001001010000001011011010000000010000

Layer 3 SDU:

[0]00 06 51 81 CA D6 80 07
[8]88 60 16 DB 62 00 43 08
[16]94 0B 68 04 00

#### o_SIB_PER_Encoding

RRC RRC @ 00:01:15.390

Category: TSO

Message Details:

Inputs:

SIB:

sIB6: (SysInfoType6)

pich_PowerOffset:-5

modeSpecificInfo:

fdd:

aich_PowerOffset:-5
dummy (CSICH_PowerOffset): Omit

primaryCCPCH_Info: Omit

prach_SystemInformationList: Omit

sCCPCH_SystemInformationList: Omit

cbs_DRX_Level1Information: Omit

nonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]00 00 00 10 10 01 00 01

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:01:15.390

Channel ID: RbBcch
Cell ID: 6

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:6

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:2
bcch_ModificationTime: Omit

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:01:15.400

Channel ID: RbBcch
Cell ID: 6

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:6

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:01:15.400

Channel ID: RbBcch
Cell ID: 6

Message Details:

RLC_TR_DATA_REQ:

cellId:6

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

completeSIB_List:

CompleteSIBshort:

sib_Type:systemInformationBlockType6
sib_Data_variable:0000001010010001

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:01:15.400

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 4

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

completeSIB_List:

CompleteSIB_List.element:

sib_Type: systemInformationBlockType6_SIB_Type [enum=6]

sib_Data_variable: 0000001010010001

Layer 3 SDU:

[0]00 0E 06 0F 02 91

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:01:15.400

Channel ID: RbBcch
Cell ID: 6

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:6

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:3
bcch_ModificationTime: Omit

#### MAC_DATA_REQ

RLC MAC @ 00:01:15.410

Category: Configuration
BTS unit: 1:2
Channel No: 0 Name: BCCH
CFN: 126

Message Details:

RLC PDU size (bits):168
RLC PDU (raw):

[0]00 0E 27 17 82 80 81 22
[8]F0 00 00 01 8B 71 80 01
[16]00 24 00 47 70

#### MAC_DATA_REQ

RLC MAC @ 00:01:15.410

Category: Configuration
BTS unit: 1:2
Channel No: 0 Name: BCCH
CFN: 126

Message Details:

RLC PDU size (bits):16
RLC PDU (raw):

[0]00 00

#### MAC_DATA_REQ

RLC MAC @ 00:01:15.410

Category: Configuration
BTS unit: 1:2
Channel No: 0 Name: BCCH
CFN: 126

Message Details:

RLC PDU size (bits):248
RLC PDU (raw):

[0]00 02 52 15 44 3E 00 FF
[8]43 FF FD D2 10 F0 29 0C
[16]0A A5 58 00 0C C5 B5 7E
[24]2B A0 FE 83 FA 0F E8

#### MAC_DATA_REQ

RLC MAC @ 00:01:15.410

Category: Configuration
BTS unit: 1:2
Channel No: 0 Name: BCCH
CFN: 126

Message Details:

RLC PDU size (bits):248
RLC PDU (raw):

[0]00 04 50 0F F4 00 00 D6
[8]34 43 F4 E5 06 10 CA 03
[16]03 81 01 60 80 E0 08 86
[24]42 99 0A 00 30 11 14

#### MAC_DATA_REQ

RLC MAC @ 00:01:15.410

Category: Configuration
BTS unit: 1:2
Channel No: 0 Name: BCCH
CFN: 126

Message Details:

RLC PDU size (bits):168
RLC PDU (raw):

[0]00 06 51 81 CA D6 80 07
[8]88 60 16 DB 62 00 43 08
[16]94 0B 68 04 00

#### PHY_DATA_REQ

MAC PHY @ 00:01:15.410

BTS unit: 1:2
Channel No: 0 Name: BCH
CFN: 126

Message Details:

SIB repetition period:64
SIB position:62
SIB size:246
SIB (raw):

[0]00 0E 27 17 82 80 81 22
[8]F0 00 00 01 8B 71 80 01
[16]00 24 00 47 70 FF F8 4C
[24]42 60 00 08 10 C2 50 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 0E 27 17 82 80 81 22
[8]F0 00 00 01 8B 71 80 01
[16]00 24 00 47 70 FF F8 4C
[24]42 60 00 08 10 C2 50

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:01:15.420

Channel ID: RbBcch
Cell ID: 6

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:6

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:01:15.420

Channel ID: RbBcch
Cell ID: 6

Message Details:

RLC_TR_DATA_REQ:

cellId:6

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

noSegment:

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:01:15.420

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 6

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

noSegment: NULL

Layer 3 SDU:

[0]00 00

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:01:15.420

Channel ID: RbBcch
Cell ID: 6

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:6

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:5
bcch_ModificationTime: Omit

#### MAC_DATA_REQ

RLC MAC @ 00:01:15.420

Category: Configuration
BTS unit: 1:2
Channel No: 0 Name: BCCH
CFN: 127

Message Details:

RLC PDU size (bits):48
RLC PDU (raw):

[0]00 0E 06 0F 02 91

#### MAC_DATA_REQ

RLC MAC @ 00:01:15.430

Category: Configuration
BTS unit: 1:2
Channel No: 0 Name: BCCH
CFN: 128

Message Details:

RLC PDU size (bits):16
RLC PDU (raw):

[0]00 00

#### PHY_DATA_REQ

MAC PHY @ 00:01:15.430

BTS unit: 1:2
Channel No: 0 Name: BCH
CFN: 128

Message Details:

SIB repetition period:64
SIB position:44
SIB size:246
SIB (raw):

[0]00 00 27 17 82 80 81 22
[8]F0 00 00 01 8B 71 80 01
[16]00 24 00 47 70 FF F8 4C
[24]42 60 00 08 10 C2 50 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 00 27 17 82 80 81 22
[8]F0 00 00 01 8B 71 80 01
[16]00 24 00 47 70 FF F8 4C
[24]42 60 00 08 10 C2 50

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:01:15.440

Channel ID: RbBcch
Cell ID: 6

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:6

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:01:15.440

Channel ID: RbBcch
Cell ID: 6

Message Details:

RLC_TR_DATA_REQ:

cellId:6

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

noSegment:

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:01:15.440

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 10

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

noSegment: NULL

Layer 3 SDU:

[0]00 00

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:01:15.440

Channel ID: RbBcch
Cell ID: 6

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:6

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:6
bcch_ModificationTime: Omit

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:01:15.450

Channel ID: RbBcch
Cell ID: 6

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:6

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:01:15.450

Channel ID: RbBcch
Cell ID: 6

Message Details:

RLC_TR_DATA_REQ:

cellId:6

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

noSegment:

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:01:15.450

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 12

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

noSegment: NULL

Layer 3 SDU:

[0]00 00

#### o_SIB_PER_Encoding

RRC RRC @ 00:01:15.450

Category: TSO

Message Details:

Inputs:

SIB:

sIB7: (SysInfoType7)

modeSpecificInfo:

fdd:

ul_Interference:-100

prach_Information_SIB5_List: (DynamicPersistenceLevelList)

DynamicPersistenceLevel:2

prach_Information_SIB6_List: (DynamicPersistenceLevelList)

DynamicPersistenceLevel:2

expirationTimeFactor: Omit

nonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]10 00 00 10 10 00 00 00
[8]10 00 00 01

#### PHY_DATA_REQ

MAC PHY @ 00:01:15.450

BTS unit: 1:2
Channel No: 0 Name: BCH
CFN: 130

Message Details:

SIB repetition period:64
SIB position:36
SIB size:246
SIB (raw):

[0]00 02 52 15 44 3E 00 FF
[8]43 FF FD D2 10 F0 29 0C
[16]0A A5 58 00 0C C5 B5 7E
[24]2B A0 FE 83 FA 0F E8 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 02 52 15 44 3E 00 FF
[8]43 FF FD D2 10 F0 29 0C
[16]0A A5 58 00 0C C5 B5 7E
[24]2B A0 FE 83 FA 0F E8

#### o_SIB_PER_Encoding

RRC RRC @ 00:01:15.470

Category: TSO

Message Details:

Inputs:

SIB:

sIB12: (SysInfoType12)

fach_MeasurementOccasionInfo: Omit

measurementControlSysInfo:

use_of_HCS:

hcs_not_used:

cellSelectQualityMeasure:

cpich_RSCP:

intraFreqMeasurementSysInfo: (IntraFreqMeasurementSysInfo_RSCP)

intraFreqMeasurementID (MeasurementIdentity): Omit

intraFreqCellInfoSI_List: (IntraFreqCellInfoSI_List_RSCP)

removedIntraFreqCellList: Omit

newIntraFreqCellList: (NewIntraFreqCellSI_List_RSCP)

NewIntraFreqCellSI_RSCP:

intraFreqCellID:7

cellInfo: (CellInfoSI_RSCP)

cellIndividualOffset: Omit

referenceTimeDifferenceToCell: Omit

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode:450

primaryCPICH_TX_Power: Omit
readSFN_Indicator:true
tx_DiversityIndicator:false

cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP)

q_OffsetS_N:0
maxAllowedUL_TX_Power:21

modeSpecificInfo:

fdd:

q_QualMin:-16
q_RxlevMin:-58

intraFreqMeasQuantity:

filterCoefficient: Omit

modeSpecificInfo:

fdd:

intraFreqMeasQuantity_FDD:cpich_RSCP

intraFreqReportingQuantityForRACH: Omit

maxReportedCellsOnRACH: Omit

reportingInfoForCellDCH:

intraFreqReportingQuantity:

activeSetReportingQuantities: (CellReportingQuantities)

dummy (SFN_SFN_OTD_Type):noReport
cellIdentity_reportingIndicator:true
cellSynchronisationInfoReportingIndicator:false

modeSpecificInfo:

fdd:

cpich_Ec_N0_reportingIndicator:false
cpich_RSCP_reportingIndicator:true
pathloss_reportingIndicator:false

monitoredSetReportingQuantities: (CellReportingQuantities)

dummy (SFN_SFN_OTD_Type):noReport
cellIdentity_reportingIndicator:true
cellSynchronisationInfoReportingIndicator:true

modeSpecificInfo:

fdd:

cpich_Ec_N0_reportingIndicator:false
cpich_RSCP_reportingIndicator:true
pathloss_reportingIndicator:false

detectedSetReportingQuantities: (CellReportingQuantities) Omit

measurementReportingMode:

measurementReportTransferMode (TransferMode):acknowledgedModeRLC
periodicalOrEventTrigger:eventTrigger

reportCriteria: (CellDCH_ReportCriteria)

intraFreqReportingCriteria:

eventCriteriaList: (IntraFreqEventCriteriaList)

IntraFreqEventCriteria:

event: (IntraFreqEvent)

e1a: (Event1a)

triggeringCondition (TriggeringCondition2):monitoredSetCellsOnly
reportingRange:5

forbiddenAffectCellList: Omit

w:1
reportDeactivationThreshold:t2
reportingAmount:ra4
reportingInterval:noPeriodicalreporting

hysteresis:0
timeToTrigger:ttt640

reportingCellStatus:

withinActiveAndOrMonitoredUsedFreq (MaxNumberOfReportingCellsType1):e3

IntraFreqEventCriteria:

event: (IntraFreqEvent)

e1b: (Event1b)

triggeringCondition (TriggeringCondition1):activeSetCellsOnly
reportingRange:5

forbiddenAffectCellList: Omit

w:1

hysteresis:0
timeToTrigger:ttt640

reportingCellStatus:

withinActiveAndOrMonitoredUsedFreq (MaxNumberOfReportingCellsType1):e3

IntraFreqEventCriteria:

event: (IntraFreqEvent)

e1c: (Event1c)

replacementActivationThreshold:t3
reportingAmount:ra4
reportingInterval:ri4

hysteresis:0
timeToTrigger:ttt640

reportingCellStatus:

withinActiveAndOrMonitoredUsedFreq (MaxNumberOfReportingCellsType1):e3

interFreqMeasurementSysInfo: (InterFreqMeasurementSysInfo_RSCP)

interFreqCellInfoSI_List: (InterFreqCellInfoSI_List_RSCP)

removedInterFreqCellList: Omit

newInterFreqCellList: (NewInterFreqCellSI_List_RSCP)

NewInterFreqCellSI_RSCP:

interFreqCellID:0

frequencyInfo:

modeSpecificInfo:

fdd: (FrequencyInfoFDD)

uarfcn_UL (UARFCN):9613
uarfcn_DL (UARFCN):10563

cellInfo: (CellInfoSI_RSCP)

cellIndividualOffset: Omit

referenceTimeDifferenceToCell: Omit

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode:100

primaryCPICH_TX_Power: Omit
readSFN_Indicator:true
tx_DiversityIndicator:false

cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP)

q_OffsetS_N:0
maxAllowedUL_TX_Power:21

modeSpecificInfo:

fdd:

q_QualMin:-16
q_RxlevMin:-58

NewInterFreqCellSI_RSCP:

interFreqCellID:1

frequencyInfo: Omit

cellInfo: (CellInfoSI_RSCP)

cellIndividualOffset: Omit

referenceTimeDifferenceToCell: Omit

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode:150

primaryCPICH_TX_Power: Omit
readSFN_Indicator:true
tx_DiversityIndicator:false

cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP)

q_OffsetS_N:0
maxAllowedUL_TX_Power:21

modeSpecificInfo:

fdd:

q_QualMin:-16
q_RxlevMin:-58

NewInterFreqCellSI_RSCP:

interFreqCellID:2

frequencyInfo: Omit

cellInfo: (CellInfoSI_RSCP)

cellIndividualOffset: Omit

referenceTimeDifferenceToCell: Omit

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode:200

primaryCPICH_TX_Power: Omit
readSFN_Indicator:true
tx_DiversityIndicator:false

cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP)

q_OffsetS_N:0
maxAllowedUL_TX_Power:21

modeSpecificInfo:

fdd:

q_QualMin:-16
q_RxlevMin:-58

NewInterFreqCellSI_RSCP:

interFreqCellID:3

frequencyInfo:

modeSpecificInfo:

fdd: (FrequencyInfoFDD)

uarfcn_UL (UARFCN):9663
uarfcn_DL (UARFCN):10613

cellInfo: (CellInfoSI_RSCP)

cellIndividualOffset: Omit

referenceTimeDifferenceToCell: Omit

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode:200

primaryCPICH_TX_Power: Omit
readSFN_Indicator:true
tx_DiversityIndicator:false

cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP)

q_OffsetS_N:0
maxAllowedUL_TX_Power:21

modeSpecificInfo:

fdd:

q_QualMin:-16
q_RxlevMin:-58

NewInterFreqCellSI_RSCP:

interFreqCellID:4

frequencyInfo: Omit

cellInfo: (CellInfoSI_RSCP)

cellIndividualOffset: Omit

referenceTimeDifferenceToCell: Omit

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode:300

primaryCPICH_TX_Power: Omit
readSFN_Indicator:true
tx_DiversityIndicator:false

cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP)

q_OffsetS_N:0
maxAllowedUL_TX_Power:21

modeSpecificInfo:

fdd:

q_QualMin:-16
q_RxlevMin:-58

NewInterFreqCellSI_RSCP:

interFreqCellID:5

frequencyInfo: Omit

cellInfo: (CellInfoSI_RSCP)

cellIndividualOffset: Omit

referenceTimeDifferenceToCell: Omit

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode:350

primaryCPICH_TX_Power: Omit
readSFN_Indicator:true
tx_DiversityIndicator:false

cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP)

q_OffsetS_N:0
maxAllowedUL_TX_Power:21

modeSpecificInfo:

fdd:

q_QualMin:-16
q_RxlevMin:-58

interRATMeasurementSysInfo: (InterRATMeasurementSysInfo_B) Omit

trafficVolumeMeasSysInfo: Omit

dummy: (UE_InternalMeasurementSysInfo) Omit

nonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]00 00 00 01 10 11 00 10
[8]00 00 01 00 11 10 01 01
[16]01 11 00 00 10 10 01 10
[24]00 11 10 01 10 10 00 00
[32]00 00 00 01 00 01 00 01
[40]00 01 10 01 00 10 10 10
[48]10 00 00 00 10 01 01 00
[56]00 10 10 01 00 00 00 00
[64]11 00 00 10 01 01 00 01
[72]00 00 01 01 00 00 10 00
[80]01 10 00 01 00 10 10 01
[88]00 11 01 01 01 00 00 11
[96]00 00 10 01 01 01 00 10
[104]11 10 00 00 01 10 01 01
[112]10 00 11 01 10 10 01 01
[120]00 00 11 00 10 10 00 11
[128]00 10 01 00 11 00 01 11
[136]00 11 01 00 00 00 00 01
[144]00 00 01 00 10 10 01 00
[152]10 11 01 00 11 00 01 11
[160]00 11 01 00 00 00 00 01
[168]00 00 10 00 10 10 01 10
[176]01 00 01 00 11 00 01 11
[184]00 11 01 00 00 00 00 01
[192]10 00 11 01 10 01 01 10
[200]11 11 11 10 10 01 01 11
[208]01 01 00 10 10 01 10 01
[216]00 01 00 11 00 01 11 00
[224]11 01 00 00 00 00 01 00
[232]01 00 00 10 10 10 01 01
[240]10 01 00 11 00 01 11 00
[248]11 01 00 00 00 00 01 00
[256]01 01 00 10 10 10 10 11
[264]11 01 00 11 00 01 11 00
[272]11 01 00 00 00 00 0

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:01:15.470

Channel ID: RbBcch
Cell ID: 6

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:6

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:15
bcch_ModificationTime: Omit

#### PHY_DATA_REQ

MAC PHY @ 00:01:15.470

BTS unit: 1:2
Channel No: 0 Name: BCH
CFN: 132

Message Details:

SIB repetition period:64
SIB position:38
SIB size:246
SIB (raw):

[0]00 04 50 0F F4 00 00 D6
[8]34 43 F4 E5 06 10 CA 03
[16]03 81 01 60 80 E0 08 86
[24]42 99 0A 00 30 11 14 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 04 50 0F F4 00 00 D6
[8]34 43 F4 E5 06 10 CA 03
[16]03 81 01 60 80 E0 08 86
[24]42 99 0A 00 30 11 14

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:01:15.480

Channel ID: RbBcch
Cell ID: 6

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:6

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:01:15.480

Channel ID: RbBcch
Cell ID: 6

Message Details:

RLC_TR_DATA_REQ:

cellId:6

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

completeSIB_List:

CompleteSIBshort:

sib_Type:systemInformationBlockType7
sib_Data_variable:100000101000000010000001

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:01:15.480

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 30

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

completeSIB_List:

CompleteSIB_List.element:

sib_Type: systemInformationBlockType7_SIB_Type [enum=7]

sib_Data_variable: 100000101000000010000001

Layer 3 SDU:

[0]00 0E 07 17 82 80 81

#### o_SIB_PER_Encoding

RRC RRC @ 00:01:15.480

Category: TSO

Message Details:

Inputs:

SIB:

sIB3: (SysInfoType3)

sib4indicator:true
cellIdentity:0000000000000000000000000110

cellSelectReselectInfo: (CellSelectReselectInfoSIB_3_4)

mappingInfo: Omit

cellSelectQualityMeasure:

cpich_RSCP:

modeSpecificInfo:

fdd:

s_Intrasearch (S_SearchQual):8
s_Intersearch (S_SearchQual):8
s_SearchHCS (S_SearchRXLEV): Omit

rat_List: (RAT_FDD_InfoList)

RAT_FDD_Info:

rat_Identifier:gsm
s_SearchRAT (S_SearchQual):-16
s_HCS_RAT (S_SearchRXLEV): Omit
s_Limit_SearchRAT (S_SearchQual):0

q_QualMin:-24
q_RxlevMin:-40

q_Hyst_l_S (Q_Hyst_S):2
t_Reselection_S:0

hcs_ServingCellInformation: Omit

maxAllowedUL_TX_Power:21

cellAccessRestriction:

cellBarred:

notBarred:

cellReservedForOperatorUse (ReservedIndicator):notReserved
cellReservationExtension (ReservedIndicator):notReserved

accessClassBarredList:

AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred

nonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]01 00 00 00 00 00 00 00
[8]00 00 00 00 00 01 10 00
[16]10 11 01 11 00 01 10 00
[24]00 00 00 00 00 01 00 00
[32]00 00 00 10 01 00 00 10
[40]00 00 01 00 01 11 11 11
[48]11 11 11 11 11 11 11 11

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:01:15.480

Channel ID: RbBcch
Cell ID: 6

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:6

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:7
bcch_ModificationTime: Omit

#### PHY_DATA_REQ

MAC PHY @ 00:01:15.490

BTS unit: 1:2
Channel No: 0 Name: BCH
CFN: 134

Message Details:

SIB repetition period:64
SIB position:42
SIB size:246
SIB (raw):

[0]00 06 51 81 CA D6 80 07
[8]88 60 16 DB 62 00 43 08
[16]94 0B 68 04 00 E0 08 86
[24]42 99 0A 00 30 11 14 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 06 51 81 CA D6 80 07
[8]88 60 16 DB 62 00 43 08
[16]94 0B 68 04 00 E0 08 86
[24]42 99 0A 00 30 11 14

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:01:15.500

Channel ID: RbBcch
Cell ID: 6

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:6

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:01:15.500

Channel ID: RbBcch
Cell ID: 6

Message Details:

RLC_TR_DATA_REQ:

cellId:6

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

completeSIB_List:

CompleteSIBshort:

sib_Type:systemInformationBlockType7
sib_Data_variable:100000101000000010000001

CompleteSIBshort:

sib_Type:systemInformationBlockType3
sib_Data_variable:0100000000000000000000000001100010110111000110000000000000010000000000100100001000000100011111111111111111111111

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:01:15.500

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 14

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

completeSIB_List:

CompleteSIB_List.element:

sib_Type: systemInformationBlockType7_SIB_Type [enum=7]

sib_Data_variable: 100000101000000010000001

CompleteSIB_List.element:

sib_Type: systemInformationBlockType3_SIB_Type [enum=3]

sib_Data_variable: 0100000000000000000000000001100010110111000110000000000000010000000000100100001000000100011111111111111111111111

Layer 3 SDU:

[0]00 0E 27 17 82 80 81 1B
[8]7A 00 00 00 C5 B8 C0 00
[16]80 12 10 23 FF FF F8

#### o_SIB_PER_Encoding

RRC RRC @ 00:01:15.500

Category: TSO

Message Details:

Inputs:

SIB:

sIB18: (SysInfoType18)

idleModePLMNIdentities: (PLMNIdentitiesOfNeighbourCells)

plmnsOfIntraFreqCellsList: Omit

plmnsOfInterFreqCellsList:

:

plmn_Identity:

mcc:

Digit:0
Digit:0
Digit:1

mnc:

Digit:0
Digit:1

:

plmn_Identity:

mcc:

Digit:0
Digit:0
Digit:1

mnc:

Digit:0
Digit:1

:

plmn_Identity:

mcc:

Digit:0
Digit:0
Digit:1

mnc:

Digit:0
Digit:1

:

plmn_Identity:

mcc:

Digit:0
Digit:0
Digit:4

mnc:

Digit:2
Digit:1

plmnsOfInterRATCellsList: Omit

connectedModePLMNIdentities: (PLMNIdentitiesOfNeighbourCells) Omit

nonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]10 00 10 00 01 11 00 00
[8]00 00 00 01 00 00 00 00
[16]11 00 00 00 00 00 01 00
[24]00 00 00 11 00 00 00 00
[32]00 01 00 00 00 00 11 00
[40]00 00 00 01 00 00 01 00
[48]00 1

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:01:15.500

Channel ID: RbBcch
Cell ID: 6

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:6

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:23
bcch_ModificationTime: Omit

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:01:15.510

Channel ID: RbBcch
Cell ID: 6

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:6

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:01:15.510

Channel ID: RbBcch
Cell ID: 6

Message Details:

RLC_TR_DATA_REQ:

cellId:6

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

completeSIB_List:

CompleteSIBshort:

sib_Type:systemInformationBlockType7
sib_Data_variable:100000101000000010000001

CompleteSIBshort:

sib_Type:systemInformationBlockType18
sib_Data_variable:100010000111000000000001000000001100000000000100000000110000000000010000000011000000000100000100001

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:01:15.510

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 46

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

completeSIB_List:

CompleteSIB_List.element:

sib_Type: systemInformationBlockType7_SIB_Type [enum=7]

sib_Data_variable: 100000101000000010000001

CompleteSIB_List.element:

sib_Type: systemInformationBlockType18_SIB_Type [enum=26]

sib_Data_variable: 100010000111000000000001000000001100000000000100000000110000000000010000000011000000000100000100001

Layer 3 SDU:

[0]00 0E 27 17 82 80 81 D3
[8]14 43 80 08 06 00 20 18
[16]00 80 60 08 21

#### o_SIB_PER_Encoding

RRC RRC @ 00:01:15.510

Category: TSO

Message Details:

Inputs:

SIB:

sIB4: (SysInfoType4)

cellIdentity:0000000000000000000000000110

cellSelectReselectInfo: (CellSelectReselectInfoSIB_3_4)

mappingInfo: Omit

cellSelectQualityMeasure:

cpich_RSCP:

modeSpecificInfo:

fdd:

s_Intrasearch (S_SearchQual):8
s_Intersearch (S_SearchQual):8
s_SearchHCS (S_SearchRXLEV): Omit

rat_List: (RAT_FDD_InfoList)

RAT_FDD_Info:

rat_Identifier:gsm
s_SearchRAT (S_SearchQual):-16
s_HCS_RAT (S_SearchRXLEV): Omit
s_Limit_SearchRAT (S_SearchQual):0

q_QualMin:-24
q_RxlevMin:-40

q_Hyst_l_S (Q_Hyst_S):0
t_Reselection_S:0

hcs_ServingCellInformation: Omit

maxAllowedUL_TX_Power:21

cellAccessRestriction:

cellBarred:

notBarred:

cellReservedForOperatorUse (ReservedIndicator):notReserved
cellReservationExtension (ReservedIndicator):notReserved

accessClassBarredList: Omit

nonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]00 00 00 00 00 00 00 00
[8]00 00 00 00 00 11 00 01
[16]01 10 11 10 00 11 00 00
[24]00 00 00 00 00 10 00 00
[32]00 00 01 00 10 00 00 00
[40]00 00 10 00 11 10 11 1

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:01:15.510

Channel ID: RbBcch
Cell ID: 6

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:6

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:31
bcch_ModificationTime: Omit

#### PHY_DATA_REQ

MAC PHY @ 00:01:15.510

BTS unit: 1:2
Channel No: 0 Name: BCH
CFN: 136

Message Details:

SIB repetition period:64
SIB position:4
SIB size:246
SIB (raw):

[0]00 0E 06 0F 02 91 80 07
[8]88 60 16 DB 62 00 43 08
[16]94 0B 68 04 00 E0 08 86
[24]42 99 0A 00 30 11 14 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 0E 06 0F 02 91 80 07
[8]88 60 16 DB 62 00 43 08
[16]94 0B 68 04 00 E0 08 86
[24]42 99 0A 00 30 11 14

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:01:15.530

Channel ID: RbBcch
Cell ID: 6

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:6

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:01:15.530

Channel ID: RbBcch
Cell ID: 6

Message Details:

RLC_TR_DATA_REQ:

cellId:6

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

completeSIB_List:

CompleteSIBshort:

sib_Type:systemInformationBlockType7
sib_Data_variable:100000101000000010000001

CompleteSIBshort:

sib_Type:systemInformationBlockType4
sib_Data_variable:00000000000000000000000000110001011011100011000000000000001000000000010010000000000010001110111

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:01:15.530

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 62

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

completeSIB_List:

CompleteSIB_List.element:

sib_Type: systemInformationBlockType7_SIB_Type [enum=7]

sib_Data_variable: 100000101000000010000001

CompleteSIB_List.element:

sib_Type: systemInformationBlockType4_SIB_Type [enum=4]

sib_Data_variable: 00000000000000000000000000110001011011100011000000000000001000000000010010000000000010001110111

Layer 3 SDU:

[0]00 0E 27 17 82 80 81 22
[8]F0 00 00 01 8B 71 80 01
[16]00 24 00 47 70

#### PHY_DATA_REQ

MAC PHY @ 00:01:15.530

BTS unit: 1:2
Channel No: 0 Name: BCH
CFN: 138

Message Details:

SIB repetition period:64
SIB position:6
SIB size:246
SIB (raw):

[0]00 00 06 0F 02 91 80 07
[8]88 60 16 DB 62 00 43 08
[16]94 0B 68 04 00 E0 08 86
[24]42 99 0A 00 30 11 14 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 00 06 0F 02 91 80 07
[8]88 60 16 DB 62 00 43 08
[16]94 0B 68 04 00 E0 08 86
[24]42 99 0A 00 30 11 14

#### o_SIB_PER_Encoding

RRC RRC @ 00:01:15.540

Category: TSO

Message Details:

Inputs:

SIB:

sIB11: (SysInfoType11)

sib12indicator:true

fach_MeasurementOccasionInfo: Omit

measurementControlSysInfo:

use_of_HCS:

hcs_not_used:

cellSelectQualityMeasure:

cpich_RSCP:

intraFreqMeasurementSysInfo: (IntraFreqMeasurementSysInfo_RSCP)

intraFreqMeasurementID (MeasurementIdentity): Omit

intraFreqCellInfoSI_List: (IntraFreqCellInfoSI_List_RSCP)

removedIntraFreqCellList: Omit

newIntraFreqCellList: (NewIntraFreqCellSI_List_RSCP)

NewIntraFreqCellSI_RSCP:

intraFreqCellID:4

cellInfo: (CellInfoSI_RSCP)

cellIndividualOffset: Omit

referenceTimeDifferenceToCell: Omit

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode:150

primaryCPICH_TX_Power: Omit
readSFN_Indicator:false
tx_DiversityIndicator:false

cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP) Omit

NewIntraFreqCellSI_RSCP:

intraFreqCellID:7

cellInfo: (CellInfoSI_RSCP)

cellIndividualOffset: Omit

referenceTimeDifferenceToCell: Omit

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode:450

primaryCPICH_TX_Power: Omit
readSFN_Indicator:true
tx_DiversityIndicator:false

cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP)

q_OffsetS_N:0
maxAllowedUL_TX_Power:21

modeSpecificInfo:

fdd:

q_QualMin:-16
q_RxlevMin:-58

intraFreqMeasQuantity:

filterCoefficient: Omit

modeSpecificInfo:

fdd:

intraFreqMeasQuantity_FDD:cpich_RSCP

intraFreqReportingQuantityForRACH: Omit

maxReportedCellsOnRACH: Omit

reportingInfoForCellDCH:

intraFreqReportingQuantity:

activeSetReportingQuantities: (CellReportingQuantities)

dummy (SFN_SFN_OTD_Type):noReport
cellIdentity_reportingIndicator:true
cellSynchronisationInfoReportingIndicator:false

modeSpecificInfo:

fdd:

cpich_Ec_N0_reportingIndicator:false
cpich_RSCP_reportingIndicator:true
pathloss_reportingIndicator:false

monitoredSetReportingQuantities: (CellReportingQuantities)

dummy (SFN_SFN_OTD_Type):noReport
cellIdentity_reportingIndicator:true
cellSynchronisationInfoReportingIndicator:true

modeSpecificInfo:

fdd:

cpich_Ec_N0_reportingIndicator:false
cpich_RSCP_reportingIndicator:true
pathloss_reportingIndicator:false

detectedSetReportingQuantities: (CellReportingQuantities) Omit

measurementReportingMode:

measurementReportTransferMode (TransferMode):acknowledgedModeRLC
periodicalOrEventTrigger:eventTrigger

reportCriteria: (CellDCH_ReportCriteria)

intraFreqReportingCriteria:

eventCriteriaList: (IntraFreqEventCriteriaList)

IntraFreqEventCriteria:

event: (IntraFreqEvent)

e1a: (Event1a)

triggeringCondition (TriggeringCondition2):monitoredSetCellsOnly
reportingRange:5

forbiddenAffectCellList: Omit

w:1
reportDeactivationThreshold:t2
reportingAmount:ra4
reportingInterval:ri4

hysteresis:0
timeToTrigger:ttt640

reportingCellStatus:

withinActiveAndOrMonitoredUsedFreq (MaxNumberOfReportingCellsType1):e3

IntraFreqEventCriteria:

event: (IntraFreqEvent)

e1b: (Event1b)

triggeringCondition (TriggeringCondition1):activeSetCellsOnly
reportingRange:5

forbiddenAffectCellList: Omit

w:1

hysteresis:0
timeToTrigger:ttt640

reportingCellStatus:

withinActiveAndOrMonitoredUsedFreq (MaxNumberOfReportingCellsType1):e3

IntraFreqEventCriteria:

event: (IntraFreqEvent)

e1c: (Event1c)

replacementActivationThreshold:t3
reportingAmount:ra4
reportingInterval:ri4

hysteresis:0
timeToTrigger:ttt640

reportingCellStatus:

withinActiveAndOrMonitoredUsedFreq (MaxNumberOfReportingCellsType1):e3

interFreqMeasurementSysInfo: (InterFreqMeasurementSysInfo_RSCP)

interFreqCellInfoSI_List: (InterFreqCellInfoSI_List_RSCP)

removedInterFreqCellList: Omit

newInterFreqCellList: (NewInterFreqCellSI_List_RSCP)

NewInterFreqCellSI_RSCP:

interFreqCellID:0

frequencyInfo:

modeSpecificInfo:

fdd: (FrequencyInfoFDD)

uarfcn_UL (UARFCN):9613
uarfcn_DL (UARFCN):10563

cellInfo: (CellInfoSI_RSCP)

cellIndividualOffset: Omit

referenceTimeDifferenceToCell: Omit

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode:100

primaryCPICH_TX_Power: Omit
readSFN_Indicator:false
tx_DiversityIndicator:false

cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP)

q_OffsetS_N:0
maxAllowedUL_TX_Power:21

modeSpecificInfo:

fdd:

q_QualMin:-16
q_RxlevMin:-58

NewInterFreqCellSI_RSCP:

interFreqCellID:1

frequencyInfo: Omit

cellInfo: (CellInfoSI_RSCP)

cellIndividualOffset: Omit

referenceTimeDifferenceToCell: Omit

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode:150

primaryCPICH_TX_Power: Omit
readSFN_Indicator:false
tx_DiversityIndicator:false

cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP)

q_OffsetS_N:0
maxAllowedUL_TX_Power:21

modeSpecificInfo:

fdd:

q_QualMin:-16
q_RxlevMin:-58

NewInterFreqCellSI_RSCP:

interFreqCellID:2

frequencyInfo: Omit

cellInfo: (CellInfoSI_RSCP)

cellIndividualOffset: Omit

referenceTimeDifferenceToCell: Omit

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode:200

primaryCPICH_TX_Power: Omit
readSFN_Indicator:false
tx_DiversityIndicator:false

cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP)

q_OffsetS_N:0
maxAllowedUL_TX_Power:21

modeSpecificInfo:

fdd:

q_QualMin:-16
q_RxlevMin:-58

NewInterFreqCellSI_RSCP:

interFreqCellID:3

frequencyInfo:

modeSpecificInfo:

fdd: (FrequencyInfoFDD)

uarfcn_UL (UARFCN):9663
uarfcn_DL (UARFCN):10613

cellInfo: (CellInfoSI_RSCP)

cellIndividualOffset: Omit

referenceTimeDifferenceToCell: Omit

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode:200

primaryCPICH_TX_Power: Omit
readSFN_Indicator:false
tx_DiversityIndicator:false

cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP)

q_OffsetS_N:0
maxAllowedUL_TX_Power:21

modeSpecificInfo:

fdd:

q_QualMin:-16
q_RxlevMin:-58

NewInterFreqCellSI_RSCP:

interFreqCellID:4

frequencyInfo: Omit

cellInfo: (CellInfoSI_RSCP)

cellIndividualOffset: Omit

referenceTimeDifferenceToCell: Omit

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode:300

primaryCPICH_TX_Power: Omit
readSFN_Indicator:false
tx_DiversityIndicator:false

cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP)

q_OffsetS_N:0
maxAllowedUL_TX_Power:21

modeSpecificInfo:

fdd:

q_QualMin:-16
q_RxlevMin:-58

NewInterFreqCellSI_RSCP:

interFreqCellID:5

frequencyInfo: Omit

cellInfo: (CellInfoSI_RSCP)

cellIndividualOffset: Omit

referenceTimeDifferenceToCell: Omit

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode:350

primaryCPICH_TX_Power: Omit
readSFN_Indicator:false
tx_DiversityIndicator:false

cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP)

q_OffsetS_N:0
maxAllowedUL_TX_Power:21

modeSpecificInfo:

fdd:

q_QualMin:-16
q_RxlevMin:-58

interRATMeasurementSysInfo: (InterRATMeasurementSysInfo_B) Omit

trafficVolumeMeasSysInfo: Omit

dummy: (UE_InternalMeasurementSysInfo) Omit

nonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]00 10 00 00 11 01 10 01
[8]00 00 01 10 01 00 00 00
[16]10 01 00 10 11 00 01 00
[24]11 10 01 01 01 11 00 00
[32]10 10 01 10 00 11 10 01
[40]10 10 00 00 00 00 00 01
[48]00 01 00 01 00 01 10 01
[56]00 10 10 10 10 00 00 00
[64]10 01 01 00 00 10 10 01
[72]01 01 00 00 11 00 00 10
[80]01 01 00 01 00 00 01 01
[88]00 00 10 00 01 10 00 01
[96]00 10 10 01 00 11 01 01
[104]01 00 00 11 00 00 10 01
[112]01 01 00 10 11 10 00 00
[120]01 10 01 01 10 00 11 01
[128]10 10 01 01 00 00 11 00
[136]10 10 00 11 00 10 00 00
[144]11 00 01 11 00 11 01 00
[152]00 00 00 01 00 00 01 00
[160]10 10 01 00 10 11 00 00
[168]11 00 01 11 00 11 01 00
[176]00 00 00 01 00 00 10 00
[184]10 10 01 10 01 00 00 00
[192]11 00 01 11 00 11 01 00
[200]00 00 00 01 10 00 11 01
[208]10 01 01 10 11 11 11 10
[216]10 01 01 11 01 01 00 10
[224]10 01 10 01 00 00 00 11
[232]00 01 11 00 11 01 00 00
[240]00 00 01 00 01 00 00 10
[248]10 10 01 01 10 00 00 11
[256]00 01 11 00 11 01 00 00
[264]00 00 01 00 01 01 00 10
[272]10 10 10 11 11 00 00 11
[280]00 01 11 00 11 01 00 00
[288]00 00 0

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:01:15.560

Channel ID: RbBcch
Cell ID: 6

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:6

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:30
bcch_ModificationTime: Omit

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:01:15.580

Channel ID: RbBcch
Cell ID: 6

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:6

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:01:15.580

Channel ID: RbBcch
Cell ID: 6

Message Details:

RLC_TR_DATA_REQ:

cellId:6

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

noSegment:

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:01:15.580

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 60

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

noSegment: NULL

Layer 3 SDU:

[0]00 00

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:01:15.580

Channel ID: RbBcch
Cell ID: 6

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:6

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:27
bcch_ModificationTime: Omit

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:01:15.590

Channel ID: RbBcch
Cell ID: 6

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:6

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:01:15.590

Channel ID: RbBcch
Cell ID: 6

Message Details:

RLC_TR_DATA_REQ:

cellId:6

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

subsequentSegment:

sib_Type:systemInformationBlockType11
segmentIndex:1
sib_Data_fixed:010101001011100000011001011000110110100101000011001010001100100000110001110011010000000001000001001010010010110000110001110011010000000001000010001010011001000000110001110011010000000001100011011001011011111110100101110101

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:01:15.590

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 54

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

subsequentSegment:

sib_Type: systemInformationBlockType11_SIB_Type [enum=11]

segmentIndex: 1

sib_Data_fixed: 010101001011100000011001011000110110100101000011001010001100100000110001110011010000000001000001001010010010110000110001110011010000000001000010001010011001000000110001110011010000000001100011011001011011111110100101110101

Layer 3 SDU:

[0]00 04 B0 54 B8 19 63 69
[8]43 28 C8 31 CD 00 41 29
[16]2C 31 CD 00 42 29 90 31
[24]CD 00 63 65 BF A5 D4

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:01:15.590

Channel ID: RbBcch
Cell ID: 6

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:6

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:26
bcch_ModificationTime: Omit

#### MAC_DATA_REQ

RLC MAC @ 00:01:15.590

Category: Configuration
BTS unit: 1:2
Channel No: 0 Name: BCCH
CFN: 144

Message Details:

RLC PDU size (bits):16
RLC PDU (raw):

[0]00 00

#### PHY_DATA_REQ

MAC PHY @ 00:01:15.590

BTS unit: 1:2
Channel No: 0 Name: BCH
CFN: 144

Message Details:

SIB repetition period:64
SIB position:10
SIB size:246
SIB (raw):

[0]00 00 06 0F 02 91 80 07
[8]88 60 16 DB 62 00 43 08
[16]94 0B 68 04 00 E0 08 86
[24]42 99 0A 00 30 11 14 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 00 06 0F 02 91 80 07
[8]88 60 16 DB 62 00 43 08
[16]94 0B 68 04 00 E0 08 86
[24]42 99 0A 00 30 11 14

#### MAC_DATA_REQ

RLC MAC @ 00:01:15.600

Category: Configuration
BTS unit: 1:2
Channel No: 0 Name: BCCH
CFN: 145

Message Details:

RLC PDU size (bits):16
RLC PDU (raw):

[0]00 00

#### MAC_DATA_REQ

RLC MAC @ 00:01:15.600

Category: Configuration
BTS unit: 1:2
Channel No: 0 Name: BCCH
CFN: 145

Message Details:

RLC PDU size (bits):56
RLC PDU (raw):

[0]00 0E 07 17 82 80 81

#### MAC_DATA_REQ

RLC MAC @ 00:01:15.600

Category: Configuration
BTS unit: 1:2
Channel No: 0 Name: BCCH
CFN: 145

Message Details:

RLC PDU size (bits):184
RLC PDU (raw):

[0]00 0E 27 17 82 80 81 1B
[8]7A 00 00 00 C5 B8 C0 00
[16]80 12 10 23 FF FF F8

#### MAC_DATA_REQ

RLC MAC @ 00:01:15.600

Category: Configuration
BTS unit: 1:2
Channel No: 0 Name: BCCH
CFN: 145

Message Details:

RLC PDU size (bits):168
RLC PDU (raw):

[0]00 0E 27 17 82 80 81 D3
[8]14 43 80 08 06 00 20 18
[16]00 80 60 08 21

#### MAC_DATA_REQ

RLC MAC @ 00:01:15.600

Category: Configuration
BTS unit: 1:2
Channel No: 0 Name: BCCH
CFN: 145

Message Details:

RLC PDU size (bits):168
RLC PDU (raw):

[0]00 0E 27 17 82 80 81 22
[8]F0 00 00 01 8B 71 80 01
[16]00 24 00 47 70

#### MAC_DATA_REQ

RLC MAC @ 00:01:15.600

Category: Configuration
BTS unit: 1:2
Channel No: 0 Name: BCCH
CFN: 145

Message Details:

RLC PDU size (bits):16
RLC PDU (raw):

[0]00 00

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:01:15.610

Channel ID: RbBcch
Cell ID: 6

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:6

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:01:15.610

Channel ID: RbBcch
Cell ID: 6

Message Details:

RLC_TR_DATA_REQ:

cellId:6

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

firstSegment:

sib_Type:systemInformationBlockType11
seg_Count (SegCount):3
sib_Data_fixed:001000001101100100000110010000001001001011000100111001010111000010100110001110011010000000000001000100010001100100101010100000001001010000101001010100001100001001010001000001010000100001100001001010010011010101000011000010

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:01:15.610

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 52

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

firstSegment:

sib_Type: systemInformationBlockType11_SIB_Type [enum=11]

seg_Count: 3

sib_Data_fixed: 001000001101100100000110010000001001001011000100111001010111000010100110001110011010000000000001000100010001100100101010100000001001010000101001010100001100001001010001000001010000100001100001001010010011010101000011000010

Layer 3 SDU:

[0]00 02 B2 20 D9 06 40 92
[8]C4 E5 70 A6 39 A0 01 11
[16]19 2A 80 94 29 50 C2 51
[24]05 08 61 29 35 43 08

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:01:15.610

Channel ID: RbBcch
Cell ID: 6

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:6

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:29
bcch_ModificationTime: Omit

#### PHY_DATA_REQ

MAC PHY @ 00:01:15.610

BTS unit: 1:2
Channel No: 0 Name: BCH
CFN: 146

Message Details:

SIB repetition period:64
SIB position:12
SIB size:246
SIB (raw):

[0]00 00 06 0F 02 91 80 07
[8]88 60 16 DB 62 00 43 08
[16]94 0B 68 04 00 E0 08 86
[24]42 99 0A 00 30 11 14 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 00 06 0F 02 91 80 07
[8]88 60 16 DB 62 00 43 08
[16]94 0B 68 04 00 E0 08 86
[24]42 99 0A 00 30 11 14

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:01:15.620

Channel ID: RbBcch
Cell ID: 6

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:6

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:01:15.620

Channel ID: RbBcch
Cell ID: 6

Message Details:

RLC_TR_DATA_REQ:

cellId:6

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

lastSegmentShort:

sib_Type:systemInformationBlockType11
segmentIndex:2
sib_Data_variable:00101001100100000011000111001101000000000100010000101010010110000011000111001101000000000100010100101010101111000011000111001101000000000

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:01:15.620

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 58

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

lastSegmentShort:

sib_Type: systemInformationBlockType11_SIB_Type [enum=11]

segmentIndex: 2

sib_Data_variable: 00101001100100000011000111001101000000000100010000101010010110000011000111001101000000000100010100101010101111000011000111001101000000000

Layer 3 SDU:

[0]00 06 B1 88 29 90 31 CD
[8]00 44 2A 58 31 CD 00 45
[16]2A BC 31 CD 00 00

#### MAC_DATA_REQ

RLC MAC @ 00:01:15.620

Category: Configuration
BTS unit: 1:2
Channel No: 0 Name: BCCH
CFN: 147

Message Details:

RLC PDU size (bits):248
RLC PDU (raw):

[0]00 04 B0 54 B8 19 63 69
[8]43 28 C8 31 CD 00 41 29
[16]2C 31 CD 00 42 29 90 31
[24]CD 00 63 65 BF A5 D4

#### MAC_DATA_REQ

RLC MAC @ 00:01:15.620

Category: Configuration
BTS unit: 1:2
Channel No: 0 Name: BCCH
CFN: 147

Message Details:

RLC PDU size (bits):248
RLC PDU (raw):

[0]00 02 B2 20 D9 06 40 92
[8]C4 E5 70 A6 39 A0 01 11
[16]19 2A 80 94 29 50 C2 51
[24]05 08 61 29 35 43 08

#### MAC_DATA_REQ

RLC MAC @ 00:01:15.630

Category: Configuration
BTS unit: 1:2
Channel No: 0 Name: BCCH
CFN: 148

Message Details:

RLC PDU size (bits):176
RLC PDU (raw):

[0]00 06 B1 88 29 90 31 CD
[8]00 44 2A 58 31 CD 00 45
[16]2A BC 31 CD 00 00

#### PHY_DATA_REQ

MAC PHY @ 00:01:15.630

BTS unit: 1:2
Channel No: 0 Name: BCH
CFN: 148

Message Details:

SIB repetition period:64
SIB position:30
SIB size:246
SIB (raw):

[0]00 0E 07 17 82 80 81 07
[8]88 60 16 DB 62 00 43 08
[16]94 0B 68 04 00 E0 08 86
[24]42 99 0A 00 30 11 14 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 0E 07 17 82 80 81 07
[8]88 60 16 DB 62 00 43 08
[16]94 0B 68 04 00 E0 08 86
[24]42 99 0A 00 30 11 14

#### o_SIB_PER_Encoding

RRC RRC @ 00:01:15.640

Category: TSO

Message Details:

Inputs:

SIB:

sIB12: (SysInfoType12)

fach_MeasurementOccasionInfo: Omit

measurementControlSysInfo:

use_of_HCS:

hcs_not_used:

cellSelectQualityMeasure:

cpich_RSCP:

intraFreqMeasurementSysInfo: (IntraFreqMeasurementSysInfo_RSCP)

intraFreqMeasurementID (MeasurementIdentity): Omit

intraFreqCellInfoSI_List: (IntraFreqCellInfoSI_List_RSCP)

removedIntraFreqCellList: Omit

newIntraFreqCellList: (NewIntraFreqCellSI_List_RSCP)

NewIntraFreqCellSI_RSCP:

intraFreqCellID:7

cellInfo: (CellInfoSI_RSCP)

cellIndividualOffset: Omit

referenceTimeDifferenceToCell: Omit

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode:450

primaryCPICH_TX_Power: Omit
readSFN_Indicator:true
tx_DiversityIndicator:false

cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP)

q_OffsetS_N:0
maxAllowedUL_TX_Power:21

modeSpecificInfo:

fdd:

q_QualMin:-16
q_RxlevMin:-58

intraFreqMeasQuantity:

filterCoefficient: Omit

modeSpecificInfo:

fdd:

intraFreqMeasQuantity_FDD:cpich_RSCP

intraFreqReportingQuantityForRACH: Omit

maxReportedCellsOnRACH: Omit

reportingInfoForCellDCH:

intraFreqReportingQuantity:

activeSetReportingQuantities: (CellReportingQuantities)

dummy (SFN_SFN_OTD_Type):noReport
cellIdentity_reportingIndicator:true
cellSynchronisationInfoReportingIndicator:false

modeSpecificInfo:

fdd:

cpich_Ec_N0_reportingIndicator:false
cpich_RSCP_reportingIndicator:true
pathloss_reportingIndicator:false

monitoredSetReportingQuantities: (CellReportingQuantities)

dummy (SFN_SFN_OTD_Type):noReport
cellIdentity_reportingIndicator:true
cellSynchronisationInfoReportingIndicator:true

modeSpecificInfo:

fdd:

cpich_Ec_N0_reportingIndicator:false
cpich_RSCP_reportingIndicator:true
pathloss_reportingIndicator:false

detectedSetReportingQuantities: (CellReportingQuantities) Omit

measurementReportingMode:

measurementReportTransferMode (TransferMode):acknowledgedModeRLC
periodicalOrEventTrigger:eventTrigger

reportCriteria: (CellDCH_ReportCriteria)

intraFreqReportingCriteria:

eventCriteriaList: (IntraFreqEventCriteriaList)

IntraFreqEventCriteria:

event: (IntraFreqEvent)

e1a: (Event1a)

triggeringCondition (TriggeringCondition2):monitoredSetCellsOnly
reportingRange:5

forbiddenAffectCellList: Omit

w:1
reportDeactivationThreshold:t2
reportingAmount:ra4
reportingInterval:noPeriodicalreporting

hysteresis:0
timeToTrigger:ttt640

reportingCellStatus:

withinActiveAndOrMonitoredUsedFreq (MaxNumberOfReportingCellsType1):e3

IntraFreqEventCriteria:

event: (IntraFreqEvent)

e1b: (Event1b)

triggeringCondition (TriggeringCondition1):activeSetCellsOnly
reportingRange:5

forbiddenAffectCellList: Omit

w:1

hysteresis:0
timeToTrigger:ttt640

reportingCellStatus:

withinActiveAndOrMonitoredUsedFreq (MaxNumberOfReportingCellsType1):e3

IntraFreqEventCriteria:

event: (IntraFreqEvent)

e1c: (Event1c)

replacementActivationThreshold:t3
reportingAmount:ra4
reportingInterval:ri4

hysteresis:0
timeToTrigger:ttt640

reportingCellStatus:

withinActiveAndOrMonitoredUsedFreq (MaxNumberOfReportingCellsType1):e3

interFreqMeasurementSysInfo: (InterFreqMeasurementSysInfo_RSCP)

interFreqCellInfoSI_List: (InterFreqCellInfoSI_List_RSCP)

removedInterFreqCellList: Omit

newInterFreqCellList: (NewInterFreqCellSI_List_RSCP)

NewInterFreqCellSI_RSCP:

interFreqCellID:0

frequencyInfo:

modeSpecificInfo:

fdd: (FrequencyInfoFDD)

uarfcn_UL (UARFCN):9613
uarfcn_DL (UARFCN):10563

cellInfo: (CellInfoSI_RSCP)

cellIndividualOffset: Omit

referenceTimeDifferenceToCell: Omit

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode:100

primaryCPICH_TX_Power: Omit
readSFN_Indicator:true
tx_DiversityIndicator:false

cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP)

q_OffsetS_N:0
maxAllowedUL_TX_Power:21

modeSpecificInfo:

fdd:

q_QualMin:-16
q_RxlevMin:-58

NewInterFreqCellSI_RSCP:

interFreqCellID:1

frequencyInfo: Omit

cellInfo: (CellInfoSI_RSCP)

cellIndividualOffset: Omit

referenceTimeDifferenceToCell: Omit

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode:150

primaryCPICH_TX_Power: Omit
readSFN_Indicator:true
tx_DiversityIndicator:false

cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP)

q_OffsetS_N:0
maxAllowedUL_TX_Power:21

modeSpecificInfo:

fdd:

q_QualMin:-16
q_RxlevMin:-58

NewInterFreqCellSI_RSCP:

interFreqCellID:2

frequencyInfo: Omit

cellInfo: (CellInfoSI_RSCP)

cellIndividualOffset: Omit

referenceTimeDifferenceToCell: Omit

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode:200

primaryCPICH_TX_Power: Omit
readSFN_Indicator:true
tx_DiversityIndicator:false

cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP)

q_OffsetS_N:0
maxAllowedUL_TX_Power:21

modeSpecificInfo:

fdd:

q_QualMin:-16
q_RxlevMin:-58

NewInterFreqCellSI_RSCP:

interFreqCellID:3

frequencyInfo:

modeSpecificInfo:

fdd: (FrequencyInfoFDD)

uarfcn_UL (UARFCN):9663
uarfcn_DL (UARFCN):10613

cellInfo: (CellInfoSI_RSCP)

cellIndividualOffset: Omit

referenceTimeDifferenceToCell: Omit

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode:200

primaryCPICH_TX_Power: Omit
readSFN_Indicator:true
tx_DiversityIndicator:false

cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP)

q_OffsetS_N:0
maxAllowedUL_TX_Power:21

modeSpecificInfo:

fdd:

q_QualMin:-16
q_RxlevMin:-58

NewInterFreqCellSI_RSCP:

interFreqCellID:4

frequencyInfo: Omit

cellInfo: (CellInfoSI_RSCP)

cellIndividualOffset: Omit

referenceTimeDifferenceToCell: Omit

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode:300

primaryCPICH_TX_Power: Omit
readSFN_Indicator:true
tx_DiversityIndicator:false

cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP)

q_OffsetS_N:0
maxAllowedUL_TX_Power:21

modeSpecificInfo:

fdd:

q_QualMin:-16
q_RxlevMin:-58

NewInterFreqCellSI_RSCP:

interFreqCellID:5

frequencyInfo: Omit

cellInfo: (CellInfoSI_RSCP)

cellIndividualOffset: Omit

referenceTimeDifferenceToCell: Omit

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode:350

primaryCPICH_TX_Power: Omit
readSFN_Indicator:true
tx_DiversityIndicator:false

cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP)

q_OffsetS_N:0
maxAllowedUL_TX_Power:21

modeSpecificInfo:

fdd:

q_QualMin:-16
q_RxlevMin:-58

interRATMeasurementSysInfo: (InterRATMeasurementSysInfo_B) Omit

trafficVolumeMeasSysInfo: Omit

dummy: (UE_InternalMeasurementSysInfo) Omit

nonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]00 00 00 01 10 11 00 10
[8]00 00 01 00 11 10 01 01
[16]01 11 00 00 10 10 01 10
[24]00 11 10 01 10 10 00 00
[32]00 00 00 01 00 01 00 01
[40]00 01 10 01 00 10 10 10
[48]10 00 00 00 10 01 01 00
[56]00 10 10 01 00 00 00 00
[64]11 00 00 10 01 01 00 01
[72]00 00 01 01 00 00 10 00
[80]01 10 00 01 00 10 10 01
[88]00 11 01 01 01 00 00 11
[96]00 00 10 01 01 01 00 10
[104]11 10 00 00 01 10 01 01
[112]10 00 11 01 10 10 01 01
[120]00 00 11 00 10 10 00 11
[128]00 10 01 00 11 00 01 11
[136]00 11 01 00 00 00 00 01
[144]00 00 01 00 10 10 01 00
[152]10 11 01 00 11 00 01 11
[160]00 11 01 00 00 00 00 01
[168]00 00 10 00 10 10 01 10
[176]01 00 01 00 11 00 01 11
[184]00 11 01 00 00 00 00 01
[192]10 00 11 01 10 01 01 10
[200]11 11 11 10 10 01 01 11
[208]01 01 00 10 10 01 10 01
[216]00 01 00 11 00 01 11 00
[224]11 01 00 00 00 00 01 00
[232]01 00 00 10 10 10 01 01
[240]10 01 00 11 00 01 11 00
[248]11 01 00 00 00 00 01 00
[256]01 01 00 10 10 10 10 11
[264]11 01 00 11 00 01 11 00
[272]11 01 00 00 00 00 0

#### PHY_DATA_REQ

MAC PHY @ 00:01:15.650

BTS unit: 1:2
Channel No: 0 Name: BCH
CFN: 150

Message Details:

SIB repetition period:64
SIB position:14
SIB size:246
SIB (raw):

[0]00 0E 27 17 82 80 81 1B
[8]7A 00 00 00 C5 B8 C0 00
[16]80 12 10 23 FF FF F8 86
[24]42 99 0A 00 30 11 14 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 0E 27 17 82 80 81 1B
[8]7A 00 00 00 C5 B8 C0 00
[16]80 12 10 23 FF FF F8 86
[24]42 99 0A 00 30 11 14

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:01:15.670

Channel ID: RbBcch
Cell ID: 6

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:6

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:13
bcch_ModificationTime: Omit

#### PHY_DATA_REQ

MAC PHY @ 00:01:15.670

BTS unit: 1:2
Channel No: 0 Name: BCH
CFN: 152

Message Details:

SIB repetition period:64
SIB position:46
SIB size:246
SIB (raw):

[0]00 0E 27 17 82 80 81 D3
[8]14 43 80 08 06 00 20 18
[16]00 80 60 08 21 FF F8 86
[24]42 99 0A 00 30 11 14 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 0E 27 17 82 80 81 D3
[8]14 43 80 08 06 00 20 18
[16]00 80 60 08 21 FF F8 86
[24]42 99 0A 00 30 11 14

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:01:15.690

Channel ID: RbBcch
Cell ID: 6

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:6

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:01:15.690

Channel ID: RbBcch
Cell ID: 6

Message Details:

RLC_TR_DATA_REQ:

cellId:6

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

subsequentSegment:

sib_Type:systemInformationBlockType12
segmentIndex:1
sib_Data_fixed:011000110110100101000011001010001100100100110001110011010000000001000001001010010010110100110001110011010000000001000010001010011001000100110001110011010000000001100011011001011011111110100101110101001010011001000100110001

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:01:15.690

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 26

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

subsequentSegment:

sib_Type: systemInformationBlockType12_SIB_Type [enum=12]

segmentIndex: 1

sib_Data_fixed: 011000110110100101000011001010001100100100110001110011010000000001000001001010010010110100110001110011010000000001000010001010011001000100110001110011010000000001100011011001011011111110100101110101001010011001000100110001

Layer 3 SDU:

[0]00 04 C0 63 69 43 28 C9
[8]31 CD 00 41 29 2D 31 CD
[16]00 42 29 91 31 CD 00 63
[24]65 BF A5 D4 A6 44 C4

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:01:15.690

Channel ID: RbBcch
Cell ID: 6

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:6

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:11
bcch_ModificationTime: Omit

#### PHY_DATA_REQ

MAC PHY @ 00:01:15.690

BTS unit: 1:2
Channel No: 0 Name: BCH
CFN: 154

Message Details:

SIB repetition period:64
SIB position:62
SIB size:246
SIB (raw):

[0]00 0E 27 17 82 80 81 22
[8]F0 00 00 01 8B 71 80 01
[16]00 24 00 47 70 FF F8 86
[24]42 99 0A 00 30 11 14 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 0E 27 17 82 80 81 22
[8]F0 00 00 01 8B 71 80 01
[16]00 24 00 47 70 FF F8 86
[24]42 99 0A 00 30 11 14

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:01:15.700

Channel ID: RbBcch
Cell ID: 6

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:6

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:01:15.700

Channel ID: RbBcch
Cell ID: 6

Message Details:

RLC_TR_DATA_REQ:

cellId:6

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

firstSegment:

sib_Type:systemInformationBlockType12
seg_Count (SegCount):3
sib_Data_fixed:000000011011001000000100111001010111000010100110001110011010000000000001000100010001100100101010100000001001010000101001000000001100001001010001000001010000100001100001001010010011010101000011000010010101001011100000011001

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:01:15.700

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 22

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

firstSegment:

sib_Type: systemInformationBlockType12_SIB_Type [enum=12]

seg_Count: 3

sib_Data_fixed: 000000011011001000000100111001010111000010100110001110011010000000000001000100010001100100101010100000001001010000101001000000001100001001010001000001010000100001100001001010010011010101000011000010010101001011100000011001

Layer 3 SDU:

[0]00 02 C2 01 B2 04 E5 70
[8]A6 39 A0 01 11 19 2A 80
[16]94 29 00 C2 51 05 08 61
[24]29 35 43 09 52 E0 64

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:01:15.700

Channel ID: RbBcch
Cell ID: 6

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:6

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:15
bcch_ModificationTime: Omit

#### PHY_DATA_REQ

MAC PHY @ 00:01:15.710

BTS unit: 1:2
Channel No: 0 Name: BCH
CFN: 156

Message Details:

SIB repetition period:64
SIB position:60
SIB size:246
SIB (raw):

[0]00 00 27 17 82 80 81 22
[8]F0 00 00 01 8B 71 80 01
[16]00 24 00 47 70 FF F8 86
[24]42 99 0A 00 30 11 14 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 00 27 17 82 80 81 22
[8]F0 00 00 01 8B 71 80 01
[16]00 24 00 47 70 FF F8 86
[24]42 99 0A 00 30 11 14

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:01:15.720

Channel ID: RbBcch
Cell ID: 6

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:6

routingInfo:

rB_Identity:-1

#### o_SIB_PER_Encoding

RRC RRC @ 00:01:15.720

Category: TSO

Message Details:

Inputs:

SIB:

sIB7: (SysInfoType7)

modeSpecificInfo:

fdd:

ul_Interference:-100

prach_Information_SIB5_List: (DynamicPersistenceLevelList)

DynamicPersistenceLevel:2

prach_Information_SIB6_List: (DynamicPersistenceLevelList)

DynamicPersistenceLevel:2

expirationTimeFactor: Omit

nonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]10 00 00 10 10 00 00 00
[8]10 00 00 01

#### RLC_TR_DATA_REQ

RRC LLA @ 00:01:15.720

Channel ID: RbBcch
Cell ID: 6

Message Details:

RLC_TR_DATA_REQ:

cellId:6

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

completeSIB_List:

CompleteSIBshort:

sib_Type:systemInformationBlockType7
sib_Data_variable:100000101000000010000001

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:01:15.720

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 30

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

completeSIB_List:

CompleteSIB_List.element:

sib_Type: systemInformationBlockType7_SIB_Type [enum=7]

sib_Data_variable: 100000101000000010000001

Layer 3 SDU:

[0]00 0E 07 17 82 80 81

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:01:15.720

Channel ID: RbBcch
Cell ID: 6

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:6

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:14
bcch_ModificationTime: Omit

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:01:15.730

Channel ID: RbBcch
Cell ID: 6

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:6

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:01:15.730

Channel ID: RbBcch
Cell ID: 6

Message Details:

RLC_TR_DATA_REQ:

cellId:6

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

lastSegmentShort:

sib_Type:systemInformationBlockType12
segmentIndex:2
sib_Data_variable:11001101000000000100010000101010010110010011000111001101000000000100010100101010101111010011000111001101000000000

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:01:15.730

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 28

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

lastSegmentShort:

sib_Type: systemInformationBlockType12_SIB_Type [enum=12]

segmentIndex: 2

sib_Data_variable: 11001101000000000100010000101010010110010011000111001101000000000100010100101010101111010011000111001101000000000

Layer 3 SDU:

[0]00 06 C1 70 CD 00 44 2A
[8]59 31 CD 00 45 2A BD 31
[16]CD 00 00

#### o_SIB_PER_Encoding

RRC RRC @ 00:01:15.730

Category: TSO

Message Details:

Inputs:

SIB:

sIB18: (SysInfoType18)

idleModePLMNIdentities: (PLMNIdentitiesOfNeighbourCells)

plmnsOfIntraFreqCellsList: Omit

plmnsOfInterFreqCellsList:

:

plmn_Identity:

mcc:

Digit:0
Digit:0
Digit:1

mnc:

Digit:0
Digit:1

:

plmn_Identity:

mcc:

Digit:0
Digit:0
Digit:1

mnc:

Digit:0
Digit:1

:

plmn_Identity:

mcc:

Digit:0
Digit:0
Digit:1

mnc:

Digit:0
Digit:1

:

plmn_Identity:

mcc:

Digit:0
Digit:0
Digit:4

mnc:

Digit:2
Digit:1

plmnsOfInterRATCellsList: Omit

connectedModePLMNIdentities: (PLMNIdentitiesOfNeighbourCells) Omit

nonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]10 00 10 00 01 11 00 00
[8]00 00 00 01 00 00 00 00
[16]11 00 00 00 00 00 01 00
[24]00 00 00 11 00 00 00 00
[32]00 01 00 00 00 00 11 00
[40]00 00 00 01 00 00 01 00
[48]00 1

#### o_SIB_PER_Encoding

RRC RRC @ 00:01:15.730

Category: TSO

Message Details:

Inputs:

SIB:

sIB7: (SysInfoType7)

modeSpecificInfo:

fdd:

ul_Interference:-100

prach_Information_SIB5_List: (DynamicPersistenceLevelList)

DynamicPersistenceLevel:2

prach_Information_SIB6_List: (DynamicPersistenceLevelList)

DynamicPersistenceLevel:2

expirationTimeFactor: Omit

nonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]10 00 00 10 10 00 00 00
[8]10 00 00 01

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:01:15.730

Channel ID: RbBcch
Cell ID: 6

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:6

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:23
bcch_ModificationTime: Omit

#### PHY_DATA_REQ

MAC PHY @ 00:01:15.730

BTS unit: 1:2
Channel No: 0 Name: BCH
CFN: 158

Message Details:

SIB repetition period:64
SIB position:54
SIB size:246
SIB (raw):

[0]00 04 B0 54 B8 19 63 69
[8]43 28 C8 31 CD 00 41 29
[16]2C 31 CD 00 42 29 90 31
[24]CD 00 63 65 BF A5 D4 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 04 B0 54 B8 19 63 69
[8]43 28 C8 31 CD 00 41 29
[16]2C 31 CD 00 42 29 90 31
[24]CD 00 63 65 BF A5 D4

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:01:15.750

Channel ID: RbBcch
Cell ID: 6

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:6

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:01:15.750

Channel ID: RbBcch
Cell ID: 6

Message Details:

RLC_TR_DATA_REQ:

cellId:6

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

completeSIB_List:

CompleteSIBshort:

sib_Type:systemInformationBlockType7
sib_Data_variable:100000101000000010000001

CompleteSIBshort:

sib_Type:systemInformationBlockType18
sib_Data_variable:100010000111000000000001000000001100000000000100000000110000000000010000000011000000000100000100001

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:01:15.750

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 46

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

completeSIB_List:

CompleteSIB_List.element:

sib_Type: systemInformationBlockType7_SIB_Type [enum=7]

sib_Data_variable: 100000101000000010000001

CompleteSIB_List.element:

sib_Type: systemInformationBlockType18_SIB_Type [enum=26]

sib_Data_variable: 100010000111000000000001000000001100000000000100000000110000000000010000000011000000000100000100001

Layer 3 SDU:

[0]00 0E 27 17 82 80 81 D3
[8]14 43 80 08 06 00 20 18
[16]00 80 60 08 21

#### o_SIB_PER_Encoding

RRC RRC @ 00:01:15.750

Category: TSO

Message Details:

Inputs:

SIB:

sB1: (SysInfoTypeSB1)

sib_ReferenceList:

SchedulingInformationSIB:

sib_Type: (SIB_TypeAndTag)

sysInfoType6 (CellValueTag):2

scheduling: (SchedulingInformation)

scheduling:

segCount: Omit

sib_Pos:

rep64:2

sib_PosOffsetInfo: (SibOFF_List) Omit

SchedulingInformationSIB:

sib_Type: (SIB_TypeAndTag)

sysInfoType7:

scheduling: (SchedulingInformation)

scheduling:

segCount: Omit

sib_Pos:

rep16:7

sib_PosOffsetInfo: (SibOFF_List) Omit

SchedulingInformationSIB:

sib_Type: (SIB_TypeAndTag)

sysInfoType11 (CellValueTag):2

scheduling: (SchedulingInformation)

scheduling:

segCount:3

sib_Pos:

rep64:26

sib_PosOffsetInfo: (SibOFF_List)

SibOFF:so2
SibOFF:so4

SchedulingInformationSIB:

sib_Type: (SIB_TypeAndTag)

sysInfoType12 (CellValueTag):2

scheduling: (SchedulingInformation)

scheduling:

segCount:3

sib_Pos:

rep64:11

sib_PosOffsetInfo: (SibOFF_List)

SibOFF:so4
SibOFF:so2

SchedulingInformationSIB:

sib_Type: (SIB_TypeAndTag)

sysInfoType18 (CellValueTag):2

scheduling: (SchedulingInformation)

scheduling:

segCount: Omit

sib_Pos:

rep64:23

sib_PosOffsetInfo: (SibOFF_List) Omit

nonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]00 01 00 00 10 10 10 00
[8]10 00 00 10 00 11 00 00
[16]01 01 11 01 01 00 11 10
[24]01 00 10 01 10 10 00 01
[32]00 00 00 01 01 01 10 11
[40]10 01 00 10 00 10 11 00
[48]01 00 01 00 00 11 00 10
[56]10 00 10 01 01 11

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:01:15.750

Channel ID: RbBcch
Cell ID: 6

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:6

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:4
sg_POS:1
bcch_ModificationTime: Omit

#### MAC_DATA_REQ

RLC MAC @ 00:01:15.750

Category: Configuration
BTS unit: 1:2
Channel No: 0 Name: BCCH
CFN: 160

Message Details:

RLC PDU size (bits):248
RLC PDU (raw):

[0]00 04 C0 63 69 43 28 C9
[8]31 CD 00 41 29 2D 31 CD
[16]00 42 29 91 31 CD 00 63
[24]65 BF A5 D4 A6 44 C4

#### MAC_DATA_REQ

RLC MAC @ 00:01:15.750

Category: Configuration
BTS unit: 1:2
Channel No: 0 Name: BCCH
CFN: 160

Message Details:

RLC PDU size (bits):248
RLC PDU (raw):

[0]00 02 C2 01 B2 04 E5 70
[8]A6 39 A0 01 11 19 2A 80
[16]94 29 00 C2 51 05 08 61
[24]29 35 43 09 52 E0 64

#### MAC_DATA_REQ

RLC MAC @ 00:01:15.750

Category: Configuration
BTS unit: 1:2
Channel No: 0 Name: BCCH
CFN: 160

Message Details:

RLC PDU size (bits):56
RLC PDU (raw):

[0]00 0E 07 17 82 80 81

#### MAC_DATA_REQ

RLC MAC @ 00:01:15.750

Category: Configuration
BTS unit: 1:2
Channel No: 0 Name: BCCH
CFN: 160

Message Details:

RLC PDU size (bits):152
RLC PDU (raw):

[0]00 06 C1 70 CD 00 44 2A
[8]59 31 CD 00 45 2A BD 31
[16]CD 00 00

#### PHY_DATA_REQ

MAC PHY @ 00:01:15.750

BTS unit: 1:2
Channel No: 0 Name: BCH
CFN: 160

Message Details:

SIB repetition period:64
SIB position:52
SIB size:246
SIB (raw):

[0]00 02 B2 20 D9 06 40 92
[8]C4 E5 70 A6 39 A0 01 11
[16]19 2A 80 94 29 50 C2 51
[24]05 08 61 29 35 43 08 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 02 B2 20 D9 06 40 92
[8]C4 E5 70 A6 39 A0 01 11
[16]19 2A 80 94 29 50 C2 51
[24]05 08 61 29 35 43 08

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:01:15.760

Channel ID: RbBcch
Cell ID: 6

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:6

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:01:15.760

Channel ID: RbBcch
Cell ID: 6

Message Details:

RLC_TR_DATA_REQ:

cellId:6

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

completeSIB_List:

CompleteSIBshort:

sib_Type:schedulingBlock1
sib_Data_variable:0001000010101000100000100011000001011101010011100100100110100001000000010101101110010010001011000100010000110010100010010111

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:01:15.760

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 16

SIB position: 2

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

completeSIB_List:

CompleteSIB_List.element:

sib_Type: schedulingBlock1_SIB_Type [enum=27]

sib_Data_variable: 0001000010101000100000100011000001011101010011100100100110100001000000010101101110010010001011000100010000110010100010010111

Layer 3 SDU:

[0]00 0E 1B 7B 10 A8 82 30
[8]5D 4E 49 A1 01 5B 92 2C
[16]44 32 89 70

#### o_SIB_PER_Encoding

RRC RRC @ 00:01:15.760

Category: TSO

Message Details:

Inputs:

SIB:

mIB: (MasterInformationBlock)

mib_ValueTag:2

plmn_Type:

gsm_MAP:

plmn_Identity:

mcc:

Digit:0
Digit:0
Digit:4

mnc:

Digit:2
Digit:1

sibSb_ReferenceList:

SchedulingInformationSIBSb:

sibSb_Type: (SIBSb_TypeAndTag)

sysInfoTypeSB1 (CellValueTag):2

scheduling: (SchedulingInformation)

scheduling:

segCount: Omit

sib_Pos:

rep16:1

sib_PosOffsetInfo: (SibOFF_List) Omit

SchedulingInformationSIBSb:

sibSb_Type: (SIBSb_TypeAndTag)

sysInfoType1 (PLMN_ValueTag):2

scheduling: (SchedulingInformation)

scheduling:

segCount: Omit

sib_Pos:

rep64:10

sib_PosOffsetInfo: (SibOFF_List) Omit

SchedulingInformationSIBSb:

sibSb_Type: (SIBSb_TypeAndTag)

sysInfoType2 (CellValueTag):2

scheduling: (SchedulingInformation)

scheduling:

segCount: Omit

sib_Pos:

rep64:10

sib_PosOffsetInfo: (SibOFF_List) Omit

SchedulingInformationSIBSb:

sibSb_Type: (SIBSb_TypeAndTag)

sysInfoType3 (CellValueTag):2

scheduling: (SchedulingInformation)

scheduling:

segCount: Omit

sib_Pos:

rep64:7

sib_PosOffsetInfo: (SibOFF_List) Omit

SchedulingInformationSIBSb:

sibSb_Type: (SIBSb_TypeAndTag)

sysInfoType4 (CellValueTag):2

scheduling: (SchedulingInformation)

scheduling:

segCount: Omit

sib_Pos:

rep64:31

sib_PosOffsetInfo: (SibOFF_List) Omit

SchedulingInformationSIBSb:

sibSb_Type: (SIBSb_TypeAndTag)

sysInfoType5 (CellValueTag):2

scheduling: (SchedulingInformation)

scheduling:

segCount:3

sib_Pos:

rep64:18

sib_PosOffsetInfo: (SibOFF_List)

SibOFF:so2
SibOFF:so4

nonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]00 01 00 00 00 00 00 01
[8]00 00 01 00 00 10 01 01
[16]10 10 10 10 00 01 00 01
[24]00 00 00 00 00 00 10 00
[32]10 00 10 10 00 00 10 10
[40]00 10 00 10 10 00 01 00
[48]10 00 10 00 01 11 00 01
[56]10 10 00 10 01 11 11 00
[64]10 00 11 10 01 00 10 01
[72]00 10 00 01 00 00 00 01

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:01:15.760

Channel ID: RbBcch
Cell ID: 6

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:6

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:3
sg_POS:0
bcch_ModificationTime: Omit

#### PHY_DATA_REQ

MAC PHY @ 00:01:15.770

BTS unit: 1:2
Channel No: 0 Name: BCH
CFN: 162

Message Details:

SIB repetition period:64
SIB position:58
SIB size:246
SIB (raw):

[0]00 06 B1 88 29 90 31 CD
[8]00 44 2A 58 31 CD 00 45
[16]2A BC 31 CD 00 00 C2 51
[24]05 08 61 29 35 43 08 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 06 B1 88 29 90 31 CD
[8]00 44 2A 58 31 CD 00 45
[16]2A BC 31 CD 00 00 C2 51
[24]05 08 61 29 35 43 08

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:01:15.780

Channel ID: RbBcch
Cell ID: 6

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:6

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:01:15.780

Channel ID: RbBcch
Cell ID: 6

Message Details:

RLC_TR_DATA_REQ:

cellId:6

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

completeSIB_List:

CompleteSIBshort:

sib_Type:masterInformationBlock
sib_Data_variable:0001000000000001000001000010010110101010000100010000000000001000100010100000101000100010100001001000100001110001101000100111110010001110010010010010000100000001

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:01:15.780

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 8

SIB position: 0

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

completeSIB_List:

CompleteSIB_List.element:

sib_Type: masterInformationBlock_SIB_Type [enum=0]

sib_Data_variable: 0001000000000001000001000010010110101010000100010000000000001000100010100000101000100010100001001000100001110001101000100111110010001110010010010010000100000001

Layer 3 SDU:

[0]00 0E 00 9F 10 01 04 25
[8]AA 11 00 08 8A 0A 22 84
[16]88 71 A2 7C 8E 49 21 01

#### PHY_DATA_REQ

MAC PHY @ 00:01:15.790

BTS unit: 1:2
Channel No: 0 Name: BCH
CFN: 164

Message Details:

SIB repetition period:64
SIB position:26
SIB size:246
SIB (raw):

[0]00 04 C0 63 69 43 28 C9
[8]31 CD 00 41 29 2D 31 CD
[16]00 42 29 91 31 CD 00 63
[24]65 BF A5 D4 A6 44 C4 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 04 C0 63 69 43 28 C9
[8]31 CD 00 41 29 2D 31 CD
[16]00 42 29 91 31 CD 00 63
[24]65 BF A5 D4 A6 44 C4

#### PHY_DATA_REQ

MAC PHY @ 00:01:15.810

BTS unit: 1:2
Channel No: 0 Name: BCH
CFN: 166

Message Details:

SIB repetition period:64
SIB position:22
SIB size:246
SIB (raw):

[0]00 02 C2 01 B2 04 E5 70
[8]A6 39 A0 01 11 19 2A 80
[16]94 29 00 C2 51 05 08 61
[24]29 35 43 09 52 E0 64 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 02 C2 01 B2 04 E5 70
[8]A6 39 A0 01 11 19 2A 80
[16]94 29 00 C2 51 05 08 61
[24]29 35 43 09 52 E0 64

#### MAC_DATA_REQ

RLC MAC @ 00:01:15.830

Category: Configuration
BTS unit: 1:2
Channel No: 0 Name: BCCH
CFN: 168

Message Details:

RLC PDU size (bits):168
RLC PDU (raw):

[0]00 0E 27 17 82 80 81 D3
[8]14 43 80 08 06 00 20 18
[16]00 80 60 08 21

#### MAC_DATA_REQ

RLC MAC @ 00:01:15.830

Category: Configuration
BTS unit: 1:2
Channel No: 0 Name: BCCH
CFN: 168

Message Details:

RLC PDU size (bits):160
RLC PDU (raw):

[0]00 0E 1B 7B 10 A8 82 30
[8]5D 4E 49 A1 01 5B 92 2C
[16]44 32 89 70

#### MAC_DATA_REQ

RLC MAC @ 00:01:15.830

Category: Configuration
BTS unit: 1:2
Channel No: 0 Name: BCCH
CFN: 168

Message Details:

RLC PDU size (bits):192
RLC PDU (raw):

[0]00 0E 00 9F 10 01 04 25
[8]AA 11 00 08 8A 0A 22 84
[16]88 71 A2 7C 8E 49 21 01

#### PHY_DATA_REQ

MAC PHY @ 00:01:15.830

BTS unit: 1:2
Channel No: 0 Name: BCH
CFN: 168

Message Details:

SIB repetition period:64
SIB position:30
SIB size:246
SIB (raw):

[0]00 0E 07 17 82 80 81 70
[8]A6 39 A0 01 11 19 2A 80
[16]94 29 00 C2 51 05 08 61
[24]29 35 43 09 52 E0 64 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 0E 07 17 82 80 81 70
[8]A6 39 A0 01 11 19 2A 80
[16]94 29 00 C2 51 05 08 61
[24]29 35 43 09 52 E0 64

#### PHY_DATA_REQ

MAC PHY @ 00:01:15.850

BTS unit: 1:2
Channel No: 0 Name: BCH
CFN: 170

Message Details:

SIB repetition period:64
SIB position:28
SIB size:246
SIB (raw):

[0]00 06 C1 70 CD 00 44 2A
[8]59 31 CD 00 45 2A BD 31
[16]CD 00 00 C2 51 05 08 61
[24]29 35 43 09 52 E0 64 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 06 C1 70 CD 00 44 2A
[8]59 31 CD 00 45 2A BD 31
[16]CD 00 00 C2 51 05 08 61
[24]29 35 43 09 52 E0 64

#### PHY_DATA_REQ

MAC PHY @ 00:01:15.870

BTS unit: 1:2
Channel No: 0 Name: BCH
CFN: 172

Message Details:

SIB repetition period:64
SIB position:46
SIB size:246
SIB (raw):

[0]00 0E 27 17 82 80 81 D3
[8]14 43 80 08 06 00 20 18
[16]00 80 60 08 21 05 08 61
[24]29 35 43 09 52 E0 64 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 0E 27 17 82 80 81 D3
[8]14 43 80 08 06 00 20 18
[16]00 80 60 08 21 05 08 61
[24]29 35 43 09 52 E0 64

#### PHY_DATA_REQ

MAC PHY @ 00:01:15.890

BTS unit: 1:2
Channel No: 0 Name: BCH
CFN: 174

Message Details:

SIB repetition period:16
SIB position:2
SIB size:246
SIB (raw):

[0]00 0E 1B 7B 10 A8 82 30
[8]5D 4E 49 A1 01 5B 92 2C
[16]44 32 89 70 21 05 08 61
[24]29 35 43 09 52 E0 64 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 0E 1B 7B 10 A8 82 30
[8]5D 4E 49 A1 01 5B 92 2C
[16]44 32 89 70 21 05 08 61
[24]29 35 43 09 52 E0 64

#### PHY_DATA_REQ

MAC PHY @ 00:01:15.910

BTS unit: 1:2
Channel No: 0 Name: BCH
CFN: 176

Message Details:

SIB repetition period:8
SIB position:0
SIB size:246
SIB (raw):

[0]00 0E 00 9F 10 01 04 25
[8]AA 11 00 08 8A 0A 22 84
[16]88 71 A2 7C 8E 49 21 01
[24]29 35 43 09 52 E0 64 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 0E 00 9F 10 01 04 25
[8]AA 11 00 08 8A 0A 22 84
[16]88 71 A2 7C 8E 49 21 01
[24]29 35 43 09 52 E0 64

#### CMAC_PAGING_Config_REQ

RRC LLA @ 00:01:20.780

Channel ID: S-CCPCH#1
Cell ID: 6

Message Details:

CMAC_PAGING_Config_REQ:

cellId:6

routingInfo:

physicalChannelIdentity:5

ratType:fdd

configMessage: (CmacPagingConfigReq)

pI_BitMapInfo:

e18:000000000000000100

dRX_CycleLength:7

iMSI: (IMSI_GSM_MAP)

Digit:0
Digit:0
Digit:1
Digit:0
Digit:1
Digit:0
Digit:0
Digit:0
Digit:0
Digit:0
Digit:0
Digit:0
Digit:3
Digit:3
Digit:3

t_pich_T_sccpch:false

#### CMAC_PAGING_Config_CNF

LLA RRC @ 00:01:20.790

Channel ID: S-CCPCH#1
Cell ID: 6

Message Details:

CMAC_PAGING_Config_CNF:

cellId:6

routingInfo:

physicalChannelIdentity:5

#### RLC_TR_DATA_REQ

RRC LLA @ 00:01:20.790

Channel ID: RbPcch
Cell ID: 6

Message Details:

RLC_TR_DATA_REQ:

cellId:6

routingInfo:

rB_Identity:-2

tM_message:

pCCH_Message:

message: (PCCH_MessageType)

pagingType1:

pagingRecordList: Omit

bcch_ModificationInfo:

mib_ValueTag:2
bcch_ModificationTime: Omit

laterNonCriticalExtensions: Omit

#### RLC_TR_DATA_REQ: pagingType1

LLA RLC @ 00:01:20.790

Channel No: 0 Name: PCCH

Message Details:

Paging Indicator: 15

DRX Cycle Length: 128

Paging Occasion: 77

PCCH_Message:

message:

pagingType1:

pagingRecordList: Omitted

bcch_ModificationInfo:

mib_ValueTag: 2

bcch_ModificationTime: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]21

#### CMAC_Config_REQ

RRC LLA @ 00:01:20.790

Channel ID: S-CCPCH#1
Cell ID: 0

Message Details:

CMAC_Config_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:5

ratType:fdd

configMessage:

reconfigure: (CmacConfigReq)

activationTime: (SS_ActivationTime)

activateNow:

uE_Info:

u_RNTI: Omit

c_RNTI: Omit

trCHInfo:

ulconnectedTrCHList: Omit

ulTFCS: (TFCS) Omit

dlconnectedTrCHList:

:

trchid (TransportChannelIdentity):12

transportChannelInfo: (CommonOrDedicatedTFS)

tti:

tti10: (CommonOrDedicatedTF_InfoList)

CommonOrDedicatedTF_Info:

tb_Size:240

numberOfTbSizeList:

NumberOfTransportBlocks:

zero:

NumberOfTransportBlocks:

one:

logicalChannelList:

allSizes:

semistaticTF_Information:

channelCodingType:

convolutional (CodingRate):half

rateMatchingAttribute:230
crc_Size:crc16

:

trchid (TransportChannelIdentity):13

transportChannelInfo: (CommonOrDedicatedTFS)

tti:

tti10: (CommonOrDedicatedTF_InfoList)

CommonOrDedicatedTF_Info:

tb_Size:168

numberOfTbSizeList:

NumberOfTransportBlocks:

zero:

NumberOfTransportBlocks:

one:

NumberOfTransportBlocks:

small:2

logicalChannelList:

allSizes:

semistaticTF_Information:

channelCodingType:

convolutional (CodingRate):half

rateMatchingAttribute:220
crc_Size:crc16

:

trchid (TransportChannelIdentity):14

transportChannelInfo: (CommonOrDedicatedTFS)

tti:

tti10: (CommonOrDedicatedTF_InfoList)

CommonOrDedicatedTF_Info:

tb_Size:360

numberOfTbSizeList:

NumberOfTransportBlocks:

zero:

NumberOfTransportBlocks:

one:

logicalChannelList:

allSizes:

semistaticTF_Information:

channelCodingType:

turbo:

rateMatchingAttribute:130
crc_Size:crc16

dlTFCS: (TFCS)

normalTFCI_Signalling: (ExplicitTFCS_Configuration)

complete: (TFCS_ReconfAdd)

ctfcSize:

ctfc4Bit:

:

ctfc4:0

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:1

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:2

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:3

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:4

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:5

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:6

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:8

powerOffsetInformation:

gainFactorInformation:

signalledGainFactors:

modeSpecificInfo:

fdd:

gainFactorBetaC (GainFactor):11

gainFactorBetaD (GainFactor):15
referenceTFC_ID:0

powerOffsetPp_m: Omit

trCH_LogCHMapping: (TrCH_LogCHMappingList1)

ulconnectedTrCHList: Omit

dlconnectedTrCHList:

:

trchid (TransportChannelIdentity):12

trCH_LogCHMappingList:

TrCH_LogicalChannelMapping:

logicalChannel_Mapping:

dl_LogicalChannelMapping: (SS_DL_LogicalChannelMapping)

macHeaderManipulation (MAC_HeaderManipulation):normalMacHeader
dl_TransportChannelType (SS_DL_TransportChannelType):pch
logicalChannelIdentity:1
logicalChannelType:pCCH

rlc_SizeList:

configured:

mac_LogicalChannelPriority:1

rB_Identity:-2
cn_DomainIdentity: Omit

:

trchid (TransportChannelIdentity):13

trCH_LogCHMappingList:

TrCH_LogicalChannelMapping:

logicalChannel_Mapping:

dl_LogicalChannelMapping: (SS_DL_LogicalChannelMapping)

macHeaderManipulation (MAC_HeaderManipulation):normalMacHeader
dl_TransportChannelType (SS_DL_TransportChannelType):fach
logicalChannelIdentity:5
logicalChannelType:cCCH

rlc_SizeList:

configured:

mac_LogicalChannelPriority:1

rB_Identity:0
cn_DomainIdentity: Omit

#### CMAC_Config_CNF

LLA RRC @ 00:01:20.810

Channel ID: S-CCPCH#1
Cell ID: 0

Message Details:

CMAC_Config_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:5

#### CMAC_Config_REQ

RRC LLA @ 00:01:20.810

Channel ID: PRACH#1
Cell ID: 0

Message Details:

CMAC_Config_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:8

ratType:fdd

configMessage:

reconfigure: (CmacConfigReq)

activationTime: (SS_ActivationTime)

activateNow:

uE_Info:

u_RNTI: Omit

c_RNTI: Omit

trCHInfo:

ulconnectedTrCHList:

:

trchid (TransportChannelIdentity):15

transportChannelInfo: (CommonOrDedicatedTFS)

tti:

tti20: (CommonOrDedicatedTF_InfoList)

CommonOrDedicatedTF_Info:

tb_Size:168

numberOfTbSizeList:

NumberOfTransportBlocks:

one:

logicalChannelList:

configured:

CommonOrDedicatedTF_Info:

tb_Size:360

numberOfTbSizeList:

NumberOfTransportBlocks:

one:

logicalChannelList:

configured:

semistaticTF_Information:

channelCodingType:

convolutional (CodingRate):half

rateMatchingAttribute:150
crc_Size:crc16

ulTFCS: (TFCS)

normalTFCI_Signalling: (ExplicitTFCS_Configuration)

complete: (TFCS_ReconfAdd)

ctfcSize:

ctfc2Bit:

:

ctfc2:0

powerOffsetInformation: Omit

:

ctfc2:1

powerOffsetInformation: Omit

dlconnectedTrCHList: Omit

dlTFCS: (TFCS) Omit

trCH_LogCHMapping: (TrCH_LogCHMappingList1)

ulconnectedTrCHList:

:

trchid (TransportChannelIdentity):15

trCH_LogCHMappingList:

TrCH_LogicalChannelMapping:

logicalChannel_Mapping:

ul_LogicalChannelMapping: (SS_UL_LogicalChannelMapping)

macHeaderManipulation (MAC_HeaderManipulation):normalMacHeader
ul_TransportChannelType (SS_UL_TransportChannelType):rach
logicalChannelIdentity:5
logicalChannelType:cCCH

rB_Identity:0
cn_DomainIdentity: Omit

dlconnectedTrCHList: Omit

#### CMAC Configuration REQ

LLA MAC @ 00:01:20.820

BTS unit: 1:2
Channel No: 0 Name: S_CCPCH
CFN: 155

Message Details:

Configuration Parameters:

Number Of Transport Channels:3

Transport Channels:

Item Number 0:

Transport Channel Parameters:

Transport Channel:

Name:PCH
Identity:0

TTI (ms):10
EP Type:1/2 Rate Convolutional Coding
CRC Size:16
RM Attribute:230
First Interleave:On
Number Of Transport Formats:2

Transport Format Set:

Transport Format 0:

Number Of Transport Blocks:0
Transport Block Size In Bits:240

Transport Format 1:

Number Of Transport Blocks:1
Transport Block Size In Bits:240

Number Of Logical Channels:1

Logical Channels:

Item Number 0:

Logical Channel:

Name:PCCH
Identity:0

Priority:1
CT Length:0
CT Value:0
TCTF Length:0
TCTF Value:0
UE ID Type:Not used
UE ID:0

Item Number 1:

Transport Channel Parameters:

Transport Channel:

Name:FACH
Identity:0

TTI (ms):10
EP Type:1/2 Rate Convolutional Coding
CRC Size:16
RM Attribute:220
First Interleave:On
Number Of Transport Formats:3

Transport Format Set:

Transport Format 0:

Number Of Transport Blocks:0
Transport Block Size In Bits:168

Transport Format 1:

Number Of Transport Blocks:1
Transport Block Size In Bits:168

Transport Format 2:

Number Of Transport Blocks:2
Transport Block Size In Bits:168

Number Of Logical Channels:1

Logical Channels:

Item Number 0:

Logical Channel:

Name:CCCH
Identity:1

Priority:1
CT Length:0
CT Value:0
TCTF Length:8
TCTF Value:64
UE ID Type:Not used
UE ID:0

Item Number 2:

Transport Channel Parameters:

Transport Channel:

Name:FACH
Identity:1

TTI (ms):10
EP Type:Turbo Coding
CRC Size:16
RM Attribute:130
First Interleave:On
Number Of Transport Formats:2

Transport Format Set:

Transport Format 0:

Number Of Transport Blocks:0
Transport Block Size In Bits:360

Transport Format 1:

Number Of Transport Blocks:1
Transport Block Size In Bits:360

Number Of Logical Channels:0

Active Flag:1

Transport Format Combination Set:

Number Of Transport Format Combinations:8

Transport Format Combinations 0:

Transport Format:0
Transport Format:0
Transport Format:0

Transport Format Combinations 1:

Transport Format:1
Transport Format:0
Transport Format:0

Transport Format Combinations 2:

Transport Format:0
Transport Format:1
Transport Format:0

Transport Format Combinations 3:

Transport Format:1
Transport Format:1
Transport Format:0

Transport Format Combinations 4:

Transport Format:0
Transport Format:2
Transport Format:0

Transport Format Combinations 5:

Transport Format:1
Transport Format:2
Transport Format:0

Transport Format Combinations 6:

Transport Format:0
Transport Format:0
Transport Format:1

Transport Format Combinations 7:

Transport Format:0
Transport Format:1
Transport Format:1

#### MAC_DATA_REQ

RLC MAC @ 00:01:20.820

Category: Configuration
BTS unit: 1:2
Channel No: 0 Name: PCCH
CFN: 155

Message Details:

RLC PDU size (bits):8
RLC PDU (raw):

[0]21

#### CMAC Configuration CNF

MAC LLA @ 00:01:20.820

BTS unit: 1:2
Channel No: 0 Name: S_CCPCH
CFN: 155

Message Details:

#### CMAC Configuration REQ

LLA MAC @ 00:01:20.830

BTS unit: 1:1
Channel No: 0 Name: PRACH
CFN: 156

Message Details:

Configuration Parameters:

Number Of Transport Channels:1

Transport Channels:

Item Number 0:

Transport Channel Parameters:

Transport Channel:

Name:RACH
Identity:0

TTI (ms):20
EP Type:1/2 Rate Convolutional Coding
CRC Size:16
RM Attribute:150
First Interleave:On
Number Of Transport Formats:2

Transport Format Set:

Transport Format 0:

Number Of Transport Blocks:1
Transport Block Size In Bits:168

Transport Format 1:

Number Of Transport Blocks:1
Transport Block Size In Bits:360

Number Of Logical Channels:1

Logical Channels:

Item Number 0:

Logical Channel:

Name:CCCH
Identity:0

Priority:0
CT Length:0
CT Value:0
TCTF Length:2
TCTF Value:0
UE ID Type:Not used
UE ID:0

Active Flag:1

Transport Format Combination Set:

Number Of Transport Format Combinations:2

Transport Format Combinations 0:

Transport Format:0

Transport Format Combinations 1:

Transport Format:1

#### CMAC Configuration CNF

MAC LLA @ 00:01:20.830

BTS unit: 1:1
Channel No: 0 Name: PRACH
CFN: 156

Message Details:

#### CMAC_Config_CNF

LLA RRC @ 00:01:20.840

Channel ID: PRACH#1
Cell ID: 0

Message Details:

CMAC_Config_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:8

#### CRLC_Config_REQ

RRC LLA @ 00:01:20.840

Channel ID: RbBcchFach
Cell ID: 0

Message Details:

CRLC_Config_REQ:

cellId:0

routingInfo:

rB_Identity:-3

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC TM Channel Release REQ

LLA RLC @ 00:01:20.850

BTS unit: 1:1
Channel No: 1 Name: BCCH
CFN: 158

Message Details:

#### CRLC TM Channel Release CNF

RLC LLA @ 00:01:20.850

BTS unit: 1:1
Channel No: 1 Name: BCCH
CFN: 158

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:01:20.860

Channel ID: RbBcchFach
Cell ID: 0

Message Details:

CRLC_Config_CNF:

cellId:0

routingInfo:

rB_Identity:-3

#### CMAC_Config_REQ

RRC LLA @ 00:01:20.860

Channel ID: S-CCPCH#1
Cell ID: 6

Message Details:

CMAC_Config_REQ:

cellId:6

routingInfo:

physicalChannelIdentity:5

ratType:fdd

configMessage:

reconfigure: (CmacConfigReq)

activationTime: (SS_ActivationTime)

activateNow:

uE_Info:

u_RNTI:

srnc_Identity:000000000001
s_RNTI:00000000000000000001

c_RNTI:0000000000000001

trCHInfo:

ulconnectedTrCHList: Omit

ulTFCS: (TFCS) Omit

dlconnectedTrCHList:

:

trchid (TransportChannelIdentity):12

transportChannelInfo: (CommonOrDedicatedTFS)

tti:

tti10: (CommonOrDedicatedTF_InfoList)

CommonOrDedicatedTF_Info:

tb_Size:240

numberOfTbSizeList:

NumberOfTransportBlocks:

zero:

NumberOfTransportBlocks:

one:

logicalChannelList:

allSizes:

semistaticTF_Information:

channelCodingType:

convolutional (CodingRate):half

rateMatchingAttribute:230
crc_Size:crc16

:

trchid (TransportChannelIdentity):13

transportChannelInfo: (CommonOrDedicatedTFS)

tti:

tti10: (CommonOrDedicatedTF_InfoList)

CommonOrDedicatedTF_Info:

tb_Size:168

numberOfTbSizeList:

NumberOfTransportBlocks:

zero:

NumberOfTransportBlocks:

one:

NumberOfTransportBlocks:

small:2

logicalChannelList:

allSizes:

semistaticTF_Information:

channelCodingType:

convolutional (CodingRate):half

rateMatchingAttribute:220
crc_Size:crc16

:

trchid (TransportChannelIdentity):14

transportChannelInfo: (CommonOrDedicatedTFS)

tti:

tti10: (CommonOrDedicatedTF_InfoList)

CommonOrDedicatedTF_Info:

tb_Size:360

numberOfTbSizeList:

NumberOfTransportBlocks:

zero:

NumberOfTransportBlocks:

one:

logicalChannelList:

allSizes:

semistaticTF_Information:

channelCodingType:

turbo:

rateMatchingAttribute:130
crc_Size:crc16

dlTFCS: (TFCS)

normalTFCI_Signalling: (ExplicitTFCS_Configuration)

complete: (TFCS_ReconfAdd)

ctfcSize:

ctfc4Bit:

:

ctfc4:0

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:1

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:2

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:3

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:4

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:5

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:6

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:8

powerOffsetInformation:

gainFactorInformation:

signalledGainFactors:

modeSpecificInfo:

fdd:

gainFactorBetaC (GainFactor):11

gainFactorBetaD (GainFactor):15
referenceTFC_ID:0

powerOffsetPp_m: Omit

trCH_LogCHMapping: (TrCH_LogCHMappingList1)

ulconnectedTrCHList: Omit

dlconnectedTrCHList:

:

trchid (TransportChannelIdentity):12

trCH_LogCHMappingList:

TrCH_LogicalChannelMapping:

logicalChannel_Mapping:

dl_LogicalChannelMapping: (SS_DL_LogicalChannelMapping)

macHeaderManipulation (MAC_HeaderManipulation):normalMacHeader
dl_TransportChannelType (SS_DL_TransportChannelType):pch
logicalChannelIdentity:1
logicalChannelType:pCCH

rlc_SizeList:

configured:

mac_LogicalChannelPriority:1

rB_Identity:-2
cn_DomainIdentity: Omit

:

trchid (TransportChannelIdentity):13

trCH_LogCHMappingList:

TrCH_LogicalChannelMapping:

logicalChannel_Mapping:

dl_LogicalChannelMapping: (SS_DL_LogicalChannelMapping)

macHeaderManipulation (MAC_HeaderManipulation):normalMacHeader
dl_TransportChannelType (SS_DL_TransportChannelType):fach
logicalChannelIdentity:6
logicalChannelType:bCCH

rlc_SizeList:

configured:

mac_LogicalChannelPriority:6

rB_Identity:-3
cn_DomainIdentity: Omit

TrCH_LogicalChannelMapping:

logicalChannel_Mapping:

dl_LogicalChannelMapping: (SS_DL_LogicalChannelMapping)

macHeaderManipulation (MAC_HeaderManipulation):normalMacHeader
dl_TransportChannelType (SS_DL_TransportChannelType):fach
logicalChannelIdentity:5
logicalChannelType:cCCH

rlc_SizeList:

configured:

mac_LogicalChannelPriority:1

rB_Identity:0
cn_DomainIdentity: Omit

TrCH_LogicalChannelMapping:

logicalChannel_Mapping:

dl_LogicalChannelMapping: (SS_DL_LogicalChannelMapping)

macHeaderManipulation (MAC_HeaderManipulation):normalMacHeader
dl_TransportChannelType (SS_DL_TransportChannelType):fach
logicalChannelIdentity:1
logicalChannelType:dCCH

rlc_SizeList:

configured:

mac_LogicalChannelPriority:1

rB_Identity:1
cn_DomainIdentity: Omit

TrCH_LogicalChannelMapping:

logicalChannel_Mapping:

dl_LogicalChannelMapping: (SS_DL_LogicalChannelMapping)

macHeaderManipulation (MAC_HeaderManipulation):normalMacHeader
dl_TransportChannelType (SS_DL_TransportChannelType):fach
logicalChannelIdentity:2
logicalChannelType:dCCH

rlc_SizeList:

configured:

mac_LogicalChannelPriority:2

rB_Identity:2
cn_DomainIdentity: Omit

TrCH_LogicalChannelMapping:

logicalChannel_Mapping:

dl_LogicalChannelMapping: (SS_DL_LogicalChannelMapping)

macHeaderManipulation (MAC_HeaderManipulation):normalMacHeader
dl_TransportChannelType (SS_DL_TransportChannelType):fach
logicalChannelIdentity:3
logicalChannelType:dCCH

rlc_SizeList:

configured:

mac_LogicalChannelPriority:3

rB_Identity:3
cn_DomainIdentity: Omit

TrCH_LogicalChannelMapping:

logicalChannel_Mapping:

dl_LogicalChannelMapping: (SS_DL_LogicalChannelMapping)

macHeaderManipulation (MAC_HeaderManipulation):normalMacHeader
dl_TransportChannelType (SS_DL_TransportChannelType):fach
logicalChannelIdentity:4
logicalChannelType:dCCH

rlc_SizeList:

configured:

mac_LogicalChannelPriority:4

rB_Identity:4
cn_DomainIdentity: Omit

:

trchid (TransportChannelIdentity):14

trCH_LogCHMappingList:

TrCH_LogicalChannelMapping:

logicalChannel_Mapping:

dl_LogicalChannelMapping: (SS_DL_LogicalChannelMapping)

macHeaderManipulation (MAC_HeaderManipulation):normalMacHeader
dl_TransportChannelType (SS_DL_TransportChannelType):fach
logicalChannelIdentity:7
logicalChannelType:dTCH

rlc_SizeList:

configured:

mac_LogicalChannelPriority:8

rB_Identity:20
cn_DomainIdentity: Omit

#### CMAC Configuration REQ

LLA MAC @ 00:01:20.880

BTS unit: 1:2
Channel No: 0 Name: S_CCPCH
CFN: 161

Message Details:

Configuration Parameters:

Number Of Transport Channels:3

Transport Channels:

Item Number 0:

Transport Channel Parameters:

Transport Channel:

Name:PCH
Identity:0

TTI (ms):10
EP Type:1/2 Rate Convolutional Coding
CRC Size:16
RM Attribute:230
First Interleave:On
Number Of Transport Formats:2

Transport Format Set:

Transport Format 0:

Number Of Transport Blocks:0
Transport Block Size In Bits:240

Transport Format 1:

Number Of Transport Blocks:1
Transport Block Size In Bits:240

Number Of Logical Channels:1

Logical Channels:

Item Number 0:

Logical Channel:

Name:PCCH
Identity:0

Priority:1
CT Length:0
CT Value:0
TCTF Length:0
TCTF Value:0
UE ID Type:Not used
UE ID:0

Item Number 1:

Transport Channel Parameters:

Transport Channel:

Name:FACH
Identity:0

TTI (ms):10
EP Type:1/2 Rate Convolutional Coding
CRC Size:16
RM Attribute:220
First Interleave:On
Number Of Transport Formats:3

Transport Format Set:

Transport Format 0:

Number Of Transport Blocks:0
Transport Block Size In Bits:168

Transport Format 1:

Number Of Transport Blocks:1
Transport Block Size In Bits:168

Transport Format 2:

Number Of Transport Blocks:2
Transport Block Size In Bits:168

Number Of Logical Channels:6

Logical Channels:

Item Number 0:

Logical Channel:

Name:BCCH
Identity:1

Priority:6
CT Length:0
CT Value:0
TCTF Length:2
TCTF Value:0
UE ID Type:Not used
UE ID:0

Item Number 1:

Logical Channel:

Name:CCCH
Identity:1

Priority:1
CT Length:0
CT Value:0
TCTF Length:8
TCTF Value:64
UE ID Type:Not used
UE ID:0

Item Number 2:

Logical Channel:

Name:DCCH
Identity:1

Priority:1
CT Length:4
CT Value:0
TCTF Length:2
TCTF Value:3
UE ID Type:C RNTI
UE ID:1

Item Number 3:

Logical Channel:

Name:DCCH
Identity:2

Priority:2
CT Length:4
CT Value:1
TCTF Length:2
TCTF Value:3
UE ID Type:C RNTI
UE ID:1

Item Number 4:

Logical Channel:

Name:DCCH
Identity:3

Priority:3
CT Length:4
CT Value:2
TCTF Length:2
TCTF Value:3
UE ID Type:C RNTI
UE ID:1

Item Number 5:

Logical Channel:

Name:DCCH
Identity:4

Priority:4
CT Length:4
CT Value:3
TCTF Length:2
TCTF Value:3
UE ID Type:C RNTI
UE ID:1

Item Number 2:

Transport Channel Parameters:

Transport Channel:

Name:FACH
Identity:1

TTI (ms):10
EP Type:Turbo Coding
CRC Size:16
RM Attribute:130
First Interleave:On
Number Of Transport Formats:2

Transport Format Set:

Transport Format 0:

Number Of Transport Blocks:0
Transport Block Size In Bits:360

Transport Format 1:

Number Of Transport Blocks:1
Transport Block Size In Bits:360

Number Of Logical Channels:1

Logical Channels:

Item Number 0:

Logical Channel:

Name:D_DTCH
Identity:4

Priority:8
CT Length:4
CT Value:6
TCTF Length:2
TCTF Value:3
UE ID Type:C RNTI
UE ID:1

Active Flag:1

Transport Format Combination Set:

Number Of Transport Format Combinations:8

Transport Format Combinations 0:

Transport Format:0
Transport Format:0
Transport Format:0

Transport Format Combinations 1:

Transport Format:1
Transport Format:0
Transport Format:0

Transport Format Combinations 2:

Transport Format:0
Transport Format:1
Transport Format:0

Transport Format Combinations 3:

Transport Format:1
Transport Format:1
Transport Format:0

Transport Format Combinations 4:

Transport Format:0
Transport Format:2
Transport Format:0

Transport Format Combinations 5:

Transport Format:1
Transport Format:2
Transport Format:0

Transport Format Combinations 6:

Transport Format:0
Transport Format:0
Transport Format:1

Transport Format Combinations 7:

Transport Format:0
Transport Format:1
Transport Format:1

#### CMAC Configuration CNF

MAC LLA @ 00:01:20.880

BTS unit: 1:2
Channel No: 0 Name: S_CCPCH
CFN: 161

Message Details:

#### CMAC_Config_CNF

LLA RRC @ 00:01:20.890

Channel ID: S-CCPCH#1
Cell ID: 6

Message Details:

CMAC_Config_CNF:

cellId:6

routingInfo:

physicalChannelIdentity:5

#### CMAC_Config_REQ

RRC LLA @ 00:01:20.890

Channel ID: PRACH#1
Cell ID: 6

Message Details:

CMAC_Config_REQ:

cellId:6

routingInfo:

physicalChannelIdentity:8

ratType:fdd

configMessage:

reconfigure: (CmacConfigReq)

activationTime: (SS_ActivationTime)

activateNow:

uE_Info:

u_RNTI: Omit

c_RNTI:0000000000000001

trCHInfo:

ulconnectedTrCHList:

:

trchid (TransportChannelIdentity):15

transportChannelInfo: (CommonOrDedicatedTFS)

tti:

tti20: (CommonOrDedicatedTF_InfoList)

CommonOrDedicatedTF_Info:

tb_Size:168

numberOfTbSizeList:

NumberOfTransportBlocks:

one:

logicalChannelList:

configured:

CommonOrDedicatedTF_Info:

tb_Size:360

numberOfTbSizeList:

NumberOfTransportBlocks:

one:

logicalChannelList:

configured:

semistaticTF_Information:

channelCodingType:

convolutional (CodingRate):half

rateMatchingAttribute:150
crc_Size:crc16

ulTFCS: (TFCS)

normalTFCI_Signalling: (ExplicitTFCS_Configuration)

complete: (TFCS_ReconfAdd)

ctfcSize:

ctfc2Bit:

:

ctfc2:0

powerOffsetInformation: Omit

:

ctfc2:1

powerOffsetInformation: Omit

dlconnectedTrCHList: Omit

dlTFCS: (TFCS) Omit

trCH_LogCHMapping: (TrCH_LogCHMappingList1)

ulconnectedTrCHList:

:

trchid (TransportChannelIdentity):15

trCH_LogCHMappingList:

TrCH_LogicalChannelMapping:

logicalChannel_Mapping:

ul_LogicalChannelMapping: (SS_UL_LogicalChannelMapping)

macHeaderManipulation (MAC_HeaderManipulation):normalMacHeader
ul_TransportChannelType (SS_UL_TransportChannelType):rach
logicalChannelIdentity:5
logicalChannelType:cCCH

rB_Identity:0
cn_DomainIdentity: Omit

TrCH_LogicalChannelMapping:

logicalChannel_Mapping:

ul_LogicalChannelMapping: (SS_UL_LogicalChannelMapping)

macHeaderManipulation (MAC_HeaderManipulation):normalMacHeader
ul_TransportChannelType (SS_UL_TransportChannelType):rach
logicalChannelIdentity:1
logicalChannelType:dCCH

rB_Identity:1
cn_DomainIdentity: Omit

TrCH_LogicalChannelMapping:

logicalChannel_Mapping:

ul_LogicalChannelMapping: (SS_UL_LogicalChannelMapping)

macHeaderManipulation (MAC_HeaderManipulation):normalMacHeader
ul_TransportChannelType (SS_UL_TransportChannelType):rach
logicalChannelIdentity:2
logicalChannelType:dCCH

rB_Identity:2
cn_DomainIdentity: Omit

TrCH_LogicalChannelMapping:

logicalChannel_Mapping:

ul_LogicalChannelMapping: (SS_UL_LogicalChannelMapping)

macHeaderManipulation (MAC_HeaderManipulation):normalMacHeader
ul_TransportChannelType (SS_UL_TransportChannelType):rach
logicalChannelIdentity:3
logicalChannelType:dCCH

rB_Identity:3
cn_DomainIdentity: Omit

TrCH_LogicalChannelMapping:

logicalChannel_Mapping:

ul_LogicalChannelMapping: (SS_UL_LogicalChannelMapping)

macHeaderManipulation (MAC_HeaderManipulation):normalMacHeader
ul_TransportChannelType (SS_UL_TransportChannelType):rach
logicalChannelIdentity:4
logicalChannelType:dCCH

rB_Identity:4
cn_DomainIdentity: Omit

TrCH_LogicalChannelMapping:

logicalChannel_Mapping:

ul_LogicalChannelMapping: (SS_UL_LogicalChannelMapping)

macHeaderManipulation (MAC_HeaderManipulation):normalMacHeader
ul_TransportChannelType (SS_UL_TransportChannelType):rach
logicalChannelIdentity:7
logicalChannelType:dTCH

rB_Identity:20
cn_DomainIdentity: Omit

dlconnectedTrCHList: Omit

#### CMAC_Config_CNF

LLA RRC @ 00:01:20.900

Channel ID: PRACH#1
Cell ID: 6

Message Details:

CMAC_Config_CNF:

cellId:6

routingInfo:

physicalChannelIdentity:8

#### CRLC_Config_REQ

RRC LLA @ 00:01:20.900

Channel ID: RbBcchFach
Cell ID: 6

Message Details:

CRLC_Config_REQ:

cellId:6

routingInfo:

rB_Identity:-3

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode) Omit

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):166

dl_RLCModeInfo: (UL_RLC_Mode)

ul_TM_RLC_Mode:

transmissionRLC_Discard: Omit

segmentationIndication:true

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity): Omit
dLlogicalChannelIdentity (LogicalChannelIdentity):6
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CMAC Configuration REQ

LLA MAC @ 00:01:20.900

BTS unit: 1:2
Channel No: 0 Name: PRACH
CFN: 163

Message Details:

Configuration Parameters:

Number Of Transport Channels:1

Transport Channels:

Item Number 0:

Transport Channel Parameters:

Transport Channel:

Name:RACH
Identity:0

TTI (ms):20
EP Type:1/2 Rate Convolutional Coding
CRC Size:16
RM Attribute:150
First Interleave:On
Number Of Transport Formats:2

Transport Format Set:

Transport Format 0:

Number Of Transport Blocks:1
Transport Block Size In Bits:168

Transport Format 1:

Number Of Transport Blocks:1
Transport Block Size In Bits:360

Number Of Logical Channels:6

Logical Channels:

Item Number 0:

Logical Channel:

Name:CCCH
Identity:0

Priority:0
CT Length:0
CT Value:0
TCTF Length:2
TCTF Value:0
UE ID Type:Not used
UE ID:0

Item Number 1:

Logical Channel:

Name:DCCH
Identity:1

Priority:0
CT Length:4
CT Value:0
TCTF Length:2
TCTF Value:1
UE ID Type:C RNTI
UE ID:1

Item Number 2:

Logical Channel:

Name:DCCH
Identity:2

Priority:0
CT Length:4
CT Value:1
TCTF Length:2
TCTF Value:1
UE ID Type:C RNTI
UE ID:1

Item Number 3:

Logical Channel:

Name:DCCH
Identity:3

Priority:0
CT Length:4
CT Value:2
TCTF Length:2
TCTF Value:1
UE ID Type:C RNTI
UE ID:1

Item Number 4:

Logical Channel:

Name:DCCH
Identity:4

Priority:0
CT Length:4
CT Value:3
TCTF Length:2
TCTF Value:1
UE ID Type:C RNTI
UE ID:1

Item Number 5:

Logical Channel:

Name:U_DTCH
Identity:4

Priority:0
CT Length:4
CT Value:6
TCTF Length:2
TCTF Value:1
UE ID Type:C RNTI
UE ID:1

Active Flag:1

Transport Format Combination Set:

Number Of Transport Format Combinations:2

Transport Format Combinations 0:

Transport Format:0

Transport Format Combinations 1:

Transport Format:1

#### CMAC Configuration CNF

MAC LLA @ 00:01:20.900

BTS unit: 1:2
Channel No: 0 Name: PRACH
CFN: 163

Message Details:

#### CRLC TM Channel Establish REQ

LLA RLC @ 00:01:20.910

BTS unit: 1:2
Channel No: 1 Name: BCCH
CFN: 164

Message Details:

Configuration Parameters:

Number Of PU Sizes:1

PU sizes In Bits:

Item 0:166

#### CRLC TM Channel Establish CNF

RLC LLA @ 00:01:20.910

BTS unit: 1:2
Channel No: 1 Name: BCCH
CFN: 164

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:01:20.920

Channel ID: RbBcchFach
Cell ID: 6

Message Details:

CRLC_Config_CNF:

cellId:6

routingInfo:

rB_Identity:-3

#### PHY_DATA_REQ

MAC PHY @ 00:01:21.340

BTS unit: 1:2
Channel No: 0 Name: PCH
CFN: 207

Message Details:

TFI:1
TB set size:240
TB size:240
TB set (raw):

[0]21 00 00 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00 00 00 00 00
[24]00 00 00 00 00 00

TB set (decoded):

TB 0:

MAC SDU (240 bits):

[0]21 00 00 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00 00 00 00 00
[24]00 00 00 00 00 00

#### PHY_DATA_IND

PHY MAC @ 00:01:43.270

BTS unit: 1:2
Channel No: 0 Name: U_RACH
CFN: 76

Message Details:

TFI:0
TB set size:168
TB size:168
TB set (raw):

[0]08 44 48 8C D1 00 04 02
[8]00 02 C0 00 00 00 00 00
[16]00 00 00 00 00 00

TB set (decoded):

TB 0:

TCTF:0
MAC SDU (166 bits):

[0]21 11 22 33 44 00 10 08
[8]00 0B 00 00 00 00 00 00
[16]00 00 00 00 00

#### MAC_DATA_IND

MAC RLC @ 00:01:43.270

Category: Configuration
BTS unit: 1:2
Channel No: 0 Name: CCCH
CFN: 76

Message Details:

RLC PDU size (bits):166
RLC PDU (raw):

[0]21 11 22 33 44 00 10 08
[8]00 0B 00 00 00 00 00 00
[16]00 00 00 00 00

#### RLC_TR_DATA_IND: rrcConnectionRequest

RLC LLA @ 00:01:43.280

Channel No: 0 Name: CCCH

Message Details:

UL_CCCH_Message:

integrityCheckInfo: Omitted

message:

rrcConnectionRequest:

initialUE_Identity:

tmsi_and_LAI:

tmsi: 00010001001000100011001101000100

lai:

plmn_Identity:

mcc:

MCC.element: 0

MCC.element: 0

MCC.element: 1

mnc:

MNC.element: 0

MNC.element: 1

lac: 0000000000000001

establishmentCause: registration_EstablishmentCause [enum=12]

protocolErrorIndicator: noError_ProtocolErrorIndicator [enum=0]

measuredResultsOnRACH: Omitted

v3d0NonCriticalExtensions: Omitted

Layer 3 SDU:

[0]21 11 22 33 44 00 10 08
[8]00 0B 00 00 00 00 00 00
[16]00 00 00 00 00

#### RLC_TR_DATA_IND

LLA RRC @ 00:01:43.280

Channel ID: Rb0
Cell ID: 6

Message Details:

RLC_TR_DATA_IND:

cellId:6

routingInfo:

rB_Identity:0

tM_message:

uL_CCCH_Message:

integrityCheckInfo: Omit

message: (UL_CCCH_MessageType)

rrcConnectionRequest:

initialUE_Identity:

tmsi_and_LAI: (TMSI_and_LAI_GSM_MAP)

tmsi (TMSI_GSM_MAP):00010001001000100011001101000100

lai:

plmn_Identity:

mcc:

Digit:0
Digit:0
Digit:1

mnc:

Digit:0
Digit:1

lac:0000000000000001

establishmentCause:registration
protocolErrorIndicator:noError

measuredResultsOnRACH: Omit

v3d0NonCriticalExtensions: Omit

#### RLC_UM_DATA_REQ

RRC LLA @ 00:01:43.280

Channel ID: Rb0
Cell ID: 6

Message Details:

RLC_UM_DATA_REQ:

cellId:6

routingInfo:

rB_Identity:0

uM_message:

dL_CCCH_Message:

integrityCheckInfo: Omit

message: (DL_CCCH_MessageType)

rrcConnectionSetup:

r3:

rrcConnectionSetup_r3: (RRCConnectionSetup_r3_IEs)

initialUE_Identity:

tmsi_and_LAI: (TMSI_and_LAI_GSM_MAP)

tmsi (TMSI_GSM_MAP):00010001001000100011001101000100

lai:

plmn_Identity:

mcc:

Digit:0
Digit:0
Digit:1

mnc:

Digit:0
Digit:1

lac:0000000000000001

rrc_TransactionIdentifier:0
activationTime: Omit

new_U_RNTI: (U_RNTI)

srnc_Identity:000000000001
s_RNTI:00000000000000000001

new_c_RNTI (C_RNTI):0000000000000001
rrc_StateIndicator:cell_FACH
utran_DRX_CycleLengthCoeff (UTRAN_DRX_CycleLengthCoefficient):9

capabilityUpdateRequirement:

ue_RadioCapabilityFDDUpdateRequirement:true
ue_RadioCapabilityTDDUpdateRequirement:false

systemSpecificCapUpdateReqList:

SystemSpecificCapUpdateReq:gsm

srb_InformationSetupList: (SRB_InformationSetupList2)

SRB_InformationSetup:

rb_Identity:1

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_UM_RLC_Mode:

transmissionRLC_Discard:

timerBasedNoExplicit (NoExplicitDiscard):dt50

dl_RLC_Mode:

dl_UM_RLC_Mode:

rb_MappingInfo:

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

rach:

logicalChannelIdentity:1

rlc_SizeList:

explicitList: (RLC_SizeExplicitList)

RLC_SizeInfo:

rlc_SizeIndex:1

mac_LogicalChannelPriority:1

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

fach:

logicalChannelIdentity:1

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

dch (TransportChannelIdentity):5

logicalChannelIdentity:1

rlc_SizeList:

configured:

mac_LogicalChannelPriority:1

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

dch (TransportChannelIdentity):10

logicalChannelIdentity:1

SRB_InformationSetup:

rb_Identity:2

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp400
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

rb_MappingInfo:

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

rach:

logicalChannelIdentity:2

rlc_SizeList:

explicitList: (RLC_SizeExplicitList)

RLC_SizeInfo:

rlc_SizeIndex:1

mac_LogicalChannelPriority:2

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

fach:

logicalChannelIdentity:2

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

dch (TransportChannelIdentity):5

logicalChannelIdentity:2

rlc_SizeList:

configured:

mac_LogicalChannelPriority:2

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

dch (TransportChannelIdentity):10

logicalChannelIdentity:2

SRB_InformationSetup:

rb_Identity:3

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp400
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

rb_MappingInfo:

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

rach:

logicalChannelIdentity:3

rlc_SizeList:

explicitList: (RLC_SizeExplicitList)

RLC_SizeInfo:

rlc_SizeIndex:1

mac_LogicalChannelPriority:3

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

fach:

logicalChannelIdentity:3

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

dch (TransportChannelIdentity):5

logicalChannelIdentity:3

rlc_SizeList:

configured:

mac_LogicalChannelPriority:3

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

dch (TransportChannelIdentity):10

logicalChannelIdentity:3

SRB_InformationSetup:

rb_Identity:4

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp400
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

rb_MappingInfo:

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

rach:

logicalChannelIdentity:4

rlc_SizeList:

explicitList: (RLC_SizeExplicitList)

RLC_SizeInfo:

rlc_SizeIndex:1

mac_LogicalChannelPriority:4

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

fach:

logicalChannelIdentity:4

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

dch (TransportChannelIdentity):5

logicalChannelIdentity:4

rlc_SizeList:

configured:

mac_LogicalChannelPriority:4

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

dch (TransportChannelIdentity):10

logicalChannelIdentity:4

ul_CommonTransChInfo:

tfc_Subset: Omit

prach_TFCS: (TFCS) Omit

modeSpecificInfo:

fdd:

ul_TFCS: (TFCS)

normalTFCI_Signalling: (ExplicitTFCS_Configuration)

complete: (TFCS_ReconfAdd)

ctfcSize:

ctfc2Bit:

:

ctfc2:0

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc2:1

powerOffsetInformation:

gainFactorInformation:

signalledGainFactors:

modeSpecificInfo:

fdd:

gainFactorBetaC (GainFactor):11

gainFactorBetaD (GainFactor):15
referenceTFC_ID:0

powerOffsetPp_m: Omit

ul_AddReconfTransChInfoList:

UL_AddReconfTransChInformation:

ul_TransportChannelType (UL_TrCH_Type):dch
transportChannelIdentity:5

transportFormatSet:

dedicatedTransChTFS:

tti:

tti40: (DedicatedDynamicTF_InfoList)

DedicatedDynamicTF_Info:

rlc_Size:

bitMode: (BitModeRLC_SizeInfo)

sizeType2:

part1:2
part2: Omit

numberOfTbSizeList:

NumberOfTransportBlocks:

zero:

NumberOfTransportBlocks:

one:

logicalChannelList:

allSizes:

semistaticTF_Information:

channelCodingType:

convolutional (CodingRate):third

rateMatchingAttribute:170
crc_Size:crc16

dl_CommonTransChInfo:

sccpch_TFCS: (TFCS) Omit

modeSpecificInfo:

fdd:

dl_Parameters:

sameAsUL:

dl_AddReconfTransChInfoList:

DL_AddReconfTransChInformation:

dl_TransportChannelType (DL_TrCH_Type):dch
dl_transportChannelIdentity (TransportChannelIdentity):10

tfs_SignallingMode:

sameAsULTrCH: (UL_TransportChannelIdentity)

ul_TransportChannelType (UL_TrCH_Type):dch
ul_TransportChannelIdentity (TransportChannelIdentity):5

dch_QualityTarget: (QualityTarget)

bler_QualityValue:-20

dummy: (TM_SignallingInfo) Omit

frequencyInfo: Omit

maxAllowedUL_TX_Power: Omit

ul_ChannelRequirement: Omit

dl_CommonInformation: Omit

dl_InformationPerRL_List: Omit

laterNonCriticalExtensions: Omit

specialLI:true

#### RLC_UM_DATA_REQ: rrcConnectionSetup

LLA RLC @ 00:01:43.280

Channel No: 1 Name: CCCH

Message Details:

DL_CCCH_Message:

integrityCheckInfo: Omitted

message:

rrcConnectionSetup:

r3:

rrcConnectionSetup_r3:

initialUE_Identity:

tmsi_and_LAI:

tmsi: 00010001001000100011001101000100

lai:

plmn_Identity:

mcc:

MCC.element: 0

MCC.element: 0

MCC.element: 1

mnc:

MNC.element: 0

MNC.element: 1

lac: 0000000000000001

rrc_TransactionIdentifier: 0

activationTime: Omitted

new_U_RNTI:

srnc_Identity: 000000000001

s_RNTI: 00000000000000000001

new_c_RNTI: 0000000000000001

rrc_StateIndicator: cell_FACH_RRC_StateIndicator [enum=1]

utran_DRX_CycleLengthCoeff: 9

capabilityUpdateRequirement:

ue_RadioCapabilityFDDUpdateRequirement: 1

ue_RadioCapabilityTDDUpdateRequirement: 0

systemSpecificCapUpdateReqList:

SystemSpecificCapUpdateReqList.element: gsm_SystemSpecificCapUpdateReq [enum=0]

srb_InformationSetupList:

SRB_InformationSetupList2.element:

rb_Identity: 1

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_UM_RLC_Mode:

transmissionRLC_Discard:

timerBasedNoExplicit: dt50_NoExplicitDiscard [enum=4]

dl_RLC_Mode:

dl_UM_RLC_Mode: NULL

rb_MappingInfo:

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

rach: NULL

logicalChannelIdentity: 1

rlc_SizeList:

explicitList:

RLC_SizeExplicitList.element:

rlc_SizeIndex: 1

mac_LogicalChannelPriority: 1

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

fach: NULL

logicalChannelIdentity: 1

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

dch: 5

logicalChannelIdentity: 1

rlc_SizeList:

configured: NULL

mac_LogicalChannelPriority: 1

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

dch: 10

logicalChannelIdentity: 1

SRB_InformationSetupList2.element:

rb_Identity: 2

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard: dat15_MaxDAT [enum=10]

transmissionWindowSize: tw32_TransmissionWindowSize [enum=3]

timerRST: tr500_TimerRST [enum=9]

max_RST: rst1_MaxRST [enum=0]

pollingInfo:

timerPollProhibit: tpp200_TimerPollProhibit [enum=19]

timerPoll: tp400_TimerPoll [enum=39]

poll_PDU: Omitted

poll_SDU: sdu1_Poll_SDU [enum=0]

lastTransmissionPDU_Poll: 1

lastRetransmissionPDU_Poll: 1

pollWindow: pw99_PollWindow [enum=7]

timerPollPeriodic: Omitted

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery: 1

receivingWindowSize: rw32_ReceivingWindowSize [enum=3]

dl_RLC_StatusInfo:

timerStatusProhibit: tsp200_TimerStatusProhibit [enum=19]

timerEPC: Omitted

missingPDU_Indicator: 1

timerStatusPeriodic: Omitted

rb_MappingInfo:

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

rach: NULL

logicalChannelIdentity: 2

rlc_SizeList:

explicitList:

RLC_SizeExplicitList.element:

rlc_SizeIndex: 1

mac_LogicalChannelPriority: 2

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

fach: NULL

logicalChannelIdentity: 2

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

dch: 5

logicalChannelIdentity: 2

rlc_SizeList:

configured: NULL

mac_LogicalChannelPriority: 2

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

dch: 10

logicalChannelIdentity: 2

SRB_InformationSetupList2.element:

rb_Identity: 3

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard: dat15_MaxDAT [enum=10]

transmissionWindowSize: tw32_TransmissionWindowSize [enum=3]

timerRST: tr500_TimerRST [enum=9]

max_RST: rst1_MaxRST [enum=0]

pollingInfo:

timerPollProhibit: tpp200_TimerPollProhibit [enum=19]

timerPoll: tp400_TimerPoll [enum=39]

poll_PDU: Omitted

poll_SDU: sdu1_Poll_SDU [enum=0]

lastTransmissionPDU_Poll: 1

lastRetransmissionPDU_Poll: 1

pollWindow: pw99_PollWindow [enum=7]

timerPollPeriodic: Omitted

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery: 1

receivingWindowSize: rw32_ReceivingWindowSize [enum=3]

dl_RLC_StatusInfo:

timerStatusProhibit: tsp200_TimerStatusProhibit [enum=19]

timerEPC: Omitted

missingPDU_Indicator: 1

timerStatusPeriodic: Omitted

rb_MappingInfo:

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

rach: NULL

logicalChannelIdentity: 3

rlc_SizeList:

explicitList:

RLC_SizeExplicitList.element:

rlc_SizeIndex: 1

mac_LogicalChannelPriority: 3

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

fach: NULL

logicalChannelIdentity: 3

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

dch: 5

logicalChannelIdentity: 3

rlc_SizeList:

configured: NULL

mac_LogicalChannelPriority: 3

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

dch: 10

logicalChannelIdentity: 3

SRB_InformationSetupList2.element:

rb_Identity: 4

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard: dat15_MaxDAT [enum=10]

transmissionWindowSize: tw32_TransmissionWindowSize [enum=3]

timerRST: tr500_TimerRST [enum=9]

max_RST: rst1_MaxRST [enum=0]

pollingInfo:

timerPollProhibit: tpp200_TimerPollProhibit [enum=19]

timerPoll: tp400_TimerPoll [enum=39]

poll_PDU: Omitted

poll_SDU: sdu1_Poll_SDU [enum=0]

lastTransmissionPDU_Poll: 1

lastRetransmissionPDU_Poll: 1

pollWindow: pw99_PollWindow [enum=7]

timerPollPeriodic: Omitted

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery: 1

receivingWindowSize: rw32_ReceivingWindowSize [enum=3]

dl_RLC_StatusInfo:

timerStatusProhibit: tsp200_TimerStatusProhibit [enum=19]

timerEPC: Omitted

missingPDU_Indicator: 1

timerStatusPeriodic: Omitted

rb_MappingInfo:

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

rach: NULL

logicalChannelIdentity: 4

rlc_SizeList:

explicitList:

RLC_SizeExplicitList.element:

rlc_SizeIndex: 1

mac_LogicalChannelPriority: 4

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

fach: NULL

logicalChannelIdentity: 4

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

dch: 5

logicalChannelIdentity: 4

rlc_SizeList:

configured: NULL

mac_LogicalChannelPriority: 4

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

dch: 10

logicalChannelIdentity: 4

ul_CommonTransChInfo:

tfc_Subset: Omitted

prach_TFCS: Omitted

modeSpecificInfo:

fdd:

ul_TFCS:

normalTFCI_Signalling:

complete:

ctfcSize:

ctfc2Bit:

ctfc2Bit.noName:

ctfc2: 0

powerOffsetInformation:

gainFactorInformation:

computedGainFactors: 0

powerOffsetPp_m: Omitted

ctfc2Bit.noName:

ctfc2: 1

powerOffsetInformation:

gainFactorInformation:

signalledGainFactors:

modeSpecificInfo:

fdd:

gainFactorBetaC: 11

gainFactorBetaD: 15

referenceTFC_ID: 0

powerOffsetPp_m: Omitted

ul_AddReconfTransChInfoList:

UL_AddReconfTransChInfoList.element:

ul_TransportChannelType: dch_UL_TrCH_Type [enum=0]

transportChannelIdentity: 5

transportFormatSet:

dedicatedTransChTFS:

tti:

tti40:

DedicatedDynamicTF_InfoList.element:

rlc_Size:

bitMode:

sizeType2:

part1: 2

part2: Omitted

numberOfTbSizeList:

numberOfTbSizeList.element:

zero: NULL

numberOfTbSizeList.element:

one: NULL

logicalChannelList:

allSizes: NULL

semistaticTF_Information:

channelCodingType:

convolutional: third_CodingRate [enum=1]

rateMatchingAttribute: 170

crc_Size: crc16_CRC_Size [enum=3]

dl_CommonTransChInfo:

sccpch_TFCS: Omitted

modeSpecificInfo:

fdd:

dl_Parameters:

sameAsUL: NULL

dl_AddReconfTransChInfoList:

DL_AddReconfTransChInfoList.element:

dl_TransportChannelType: dch_DL_TrCH_Type [enum=0]

dl_transportChannelIdentity: 10

tfs_SignallingMode:

sameAsULTrCH:

ul_TransportChannelType: dch_UL_TrCH_Type [enum=0]

ul_TransportChannelIdentity: 5

dch_QualityTarget:

bler_QualityValue: -20

dummy: Omitted

frequencyInfo: Omitted

maxAllowedUL_TX_Power: Omitted

ul_ChannelRequirement: Omitted

dl_CommonInformation: Omitted

dl_InformationPerRL_List: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]31 E0 22 24 46 68 80 02
[8]01 00 01 00 04 00 00 40
[16]00 5D 83 03 6A 27 50 80
[24]00 A1 A1 01 08 90 85 9E
[32]8E 46 C9 CE 7C 9C 4E 75
[40]18 00 2A 3A 10 52 89 18
[48]99 E8 E4 6C 9C E7 C9 C4
[56]E7 52 80 04 A5 A1 09 48
[64]92 8D 9E 8E 46 C9 CE 7C
[72]9C 4E 75 38 00 6A 7A 10
[80]D6 89 32 00 01 89 4A FC
[88]00 84 02 20 88 EA 59 82
[96]26 25 60

#### MAC_DATA_REQ

RLC MAC @ 00:01:43.310

Category: Configuration
BTS unit: 1:2
Channel No: 1 Name: CCCH
CFN: 100

Message Details:

RLC PDU size (bits):160
RLC PDU (raw):

[0]01 F8 31 E0 22 24 46 68
[8]80 02 01 00 01 00 04 00
[16]00 40 00 5D

RLC PDU (decoded):

Sequence number:0
Length indicator 0 (octets):124 (the first data octet in this RLC PDU is the first octet of a RLC SDU)
Segment associated with length indicator 0 (0 octets):

Last segment, not associated with any length indicators (18 octets):

[0]31 E0 22 24 46 68 80 02
[8]01 00 01 00 04 00 00 40
[16]00 5D

#### MAC_DATA_REQ

RLC MAC @ 00:01:43.310

Category: Configuration
BTS unit: 1:2
Channel No: 1 Name: CCCH
CFN: 100

Message Details:

RLC PDU size (bits):160
RLC PDU (raw):

[0]02 83 03 6A 27 50 80 00
[8]A1 A1 01 08 90 85 9E 8E
[16]46 C9 CE 7C

RLC PDU (decoded):

Sequence number:1
Last segment, not associated with any length indicators (19 octets):

[0]83 03 6A 27 50 80 00 A1
[8]A1 01 08 90 85 9E 8E 46
[16]C9 CE 7C

#### MAC_DATA_REQ

RLC MAC @ 00:01:43.310

Category: Configuration
BTS unit: 1:2
Channel No: 1 Name: CCCH
CFN: 100

Message Details:

RLC PDU size (bits):160
RLC PDU (raw):

[0]04 9C 4E 75 18 00 2A 3A
[8]10 52 89 18 99 E8 E4 6C
[16]9C E7 C9 C4

RLC PDU (decoded):

Sequence number:2
Last segment, not associated with any length indicators (19 octets):

[0]9C 4E 75 18 00 2A 3A 10
[8]52 89 18 99 E8 E4 6C 9C
[16]E7 C9 C4

#### MAC_DATA_REQ

RLC MAC @ 00:01:43.310

Category: Configuration
BTS unit: 1:2
Channel No: 1 Name: CCCH
CFN: 100

Message Details:

RLC PDU size (bits):160
RLC PDU (raw):

[0]06 E7 52 80 04 A5 A1 09
[8]48 92 8D 9E 8E 46 C9 CE
[16]7C 9C 4E 75

RLC PDU (decoded):

Sequence number:3
Last segment, not associated with any length indicators (19 octets):

[0]E7 52 80 04 A5 A1 09 48
[8]92 8D 9E 8E 46 C9 CE 7C
[16]9C 4E 75

#### MAC_DATA_REQ

RLC MAC @ 00:01:43.310

Category: Configuration
BTS unit: 1:2
Channel No: 1 Name: CCCH
CFN: 100

Message Details:

RLC PDU size (bits):160
RLC PDU (raw):

[0]08 38 00 6A 7A 10 D6 89
[8]32 00 01 89 4A FC 00 84
[16]02 20 88 EA

RLC PDU (decoded):

Sequence number:4
Last segment, not associated with any length indicators (19 octets):

[0]38 00 6A 7A 10 D6 89 32
[8]00 01 89 4A FC 00 84 02
[16]20 88 EA

#### MAC_DATA_REQ

RLC MAC @ 00:01:43.310

Category: Configuration
BTS unit: 1:2
Channel No: 1 Name: CCCH
CFN: 100

Message Details:

RLC PDU size (bits):160
RLC PDU (raw):

[0]0B 0B FE 59 82 26 25 60
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

RLC PDU (decoded):

Sequence number:5
Length indicator 0 (octets):5
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (5 octets):

[0]59 82 26 25 60
Padding associated with length indicator 1 (12 octets):

[0]00 00 00 00 00 00 00 00
[8]00 00 00 00

#### PHY_DATA_REQ

MAC PHY @ 00:01:43.310

BTS unit: 1:2
Channel No: 0 Name: FACH
CFN: 100

Message Details:

TFI:2
TB set size:336
TB size:168
TB set (raw, each TB word aligned):

[0]40 01 F8 31 E0 22 24 46
[8]68 80 02 01 00 01 00 04
[16]00 00 40 00 5D 00 40 02
[24]83 03 6A 27 50 80 00 A1
[32]A1 01 08 90 85 9E 8E 46
[40]C9 CE 7C 00

TB set (decoded):

TB 0:

TCTF:64
MAC SDU (160 bits):

[0]01 F8 31 E0 22 24 46 68
[8]80 02 01 00 01 00 04 00
[16]00 40 00 5D

TB 1:

TCTF:64
MAC SDU (160 bits):

[0]02 83 03 6A 27 50 80 00
[8]A1 A1 01 08 90 85 9E 8E
[16]46 C9 CE 7C

#### PHY_DATA_REQ

MAC PHY @ 00:01:43.320

BTS unit: 1:2
Channel No: 0 Name: FACH
CFN: 101

Message Details:

TFI:2
TB set size:336
TB size:168
TB set (raw, each TB word aligned):

[0]40 04 9C 4E 75 18 00 2A
[8]3A 10 52 89 18 99 E8 E4
[16]6C 9C E7 C9 C4 00 40 06
[24]E7 52 80 04 A5 A1 09 48
[32]92 8D 9E 8E 46 C9 CE 7C
[40]9C 4E 75 00

TB set (decoded):

TB 0:

TCTF:64
MAC SDU (160 bits):

[0]04 9C 4E 75 18 00 2A 3A
[8]10 52 89 18 99 E8 E4 6C
[16]9C E7 C9 C4

TB 1:

TCTF:64
MAC SDU (160 bits):

[0]06 E7 52 80 04 A5 A1 09
[8]48 92 8D 9E 8E 46 C9 CE
[16]7C 9C 4E 75

#### PHY_DATA_REQ

MAC PHY @ 00:01:43.330

BTS unit: 1:2
Channel No: 0 Name: FACH
CFN: 102

Message Details:

TFI:2
TB set size:336
TB size:168
TB set (raw, each TB word aligned):

[0]40 08 38 00 6A 7A 10 D6
[8]89 32 00 01 89 4A FC 00
[16]84 02 20 88 EA 00 40 0B
[24]0B FE 59 82 26 25 60 00
[32]00 00 00 00 00 00 00 00
[40]00 00 00 00

TB set (decoded):

TB 0:

TCTF:64
MAC SDU (160 bits):

[0]08 38 00 6A 7A 10 D6 89
[8]32 00 01 89 4A FC 00 84
[16]02 20 88 EA

TB 1:

TCTF:64
MAC SDU (160 bits):

[0]0B 0B FE 59 82 26 25 60
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

#### PHY_DATA_IND

PHY MAC @ 00:01:43.760

BTS unit: 1:2
Channel No: 0 Name: U_RACH
CFN: 125

Message Details:

TFI:0
TB set size:168
TB size:168
TB set (raw):

[0]50 00 11 80 00 4A 0C 00
[8]00 80 00 05 E2 34 1A 20
[16]90 98 CD 08 C5 00

TB set (decoded):

TB 0:

TCTF:1
UEID type:C-RNTI
UEID:1
C/T:1
MAC SDU (144 bits):

[0]80 00 4A 0C 00 00 80 00
[8]05 E2 34 1A 20 90 98 CD
[16]08 C5

#### MAC_DATA_IND

MAC RLC @ 00:01:43.760

Category: Configuration
BTS unit: 1:2
Channel No: 2 Name: DCCH
CFN: 125

Message Details:

RLC PDU size (bits):142
RLC PDU (raw):

[0]80 00 4A 0C 00 00 80 00
[8]05 E2 34 1A 20 90 98 CD
[16]08 C5

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:0
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]4A 0C 00 00 80 00 05 E2
[8]34 1A 20 90 98 CD 08 C5

#### PHY_DATA_IND

PHY MAC @ 00:01:43.820

BTS unit: 1:2
Channel No: 0 Name: U_RACH
CFN: 131

Message Details:

TFI:0
TB set size:168
TB size:168
TB set (raw):

[0]50 00 11 80 0D 15 FE 92
[8]60 41 00 01 00 02 31 F1
[16]F0 55 55 55 55 00

TB set (decoded):

TB 0:

TCTF:1
UEID type:C-RNTI
UEID:1
C/T:1
MAC SDU (144 bits):

[0]80 0D 15 FE 92 60 41 00
[8]01 00 02 31 F1 F0 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:01:43.820

Category: Configuration
BTS unit: 1:2
Channel No: 2 Name: DCCH
CFN: 131

Message Details:

RLC PDU size (bits):142
RLC PDU (raw):

[0]80 0D 15 FE 92 60 41 00
[8]01 00 02 31 F1 F0 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:1
Polling bit:1 (request a status report)
Length indicator 0 (octets):10
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (10 octets):

[0]92 60 41 00 01 00 02 31
[8]F1 F0
Padding associated with length indicator 1 (4 octets):

[0]55 55 55 55

#### MAC_DATA_REQ

RLC MAC @ 00:01:43.830

Category: Configuration
BTS unit: 1:2
Channel No: 2 Name: DCCH
CFN: 152

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 20 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:2

#### PHY_DATA_REQ

MAC PHY @ 00:01:43.830

BTS unit: 1:2
Channel No: 0 Name: FACH
CFN: 152

Message Details:

TFI:1
TB set size:168
TB size:168
TB set (raw):

[0]D0 00 11 02 00 20 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00 00 00

TB set (decoded):

TB 0:

TCTF:3
UEID type:C-RNTI
UEID:1
C/T:1
MAC SDU (144 bits):

[0]02 00 20 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### RLC_AM_DATA_IND: rrcConnectionSetupComplete

RLC LLA @ 00:01:43.840

Channel No: 2 Name: DCCH

Message Details:

UL_DCCH_Message:

integrityCheckInfo: Omitted

message:

rrcConnectionSetupComplete:

rrc_TransactionIdentifier: 0

startList:

STARTList.element:

cn_DomainIdentity: ps_domain_CN_DomainIdentity [enum=1]

start_Value: 00000000000000000010

STARTList.element:

cn_DomainIdentity: cs_domain_CN_DomainIdentity [enum=0]

start_Value: 00000000000000000010

ue_RadioAccessCapability:

accessStratumReleaseIndicator: r99_AccessStratumReleaseIndicator [enum=0]

pdcp_Capability:

losslessSRNS_RelocationSupport: 1

supportForRfc2507:

supported: by8192_MaxHcContextSpace [enum=4]

rlc_Capability:

totalRLC_AM_BufferSize: kb50_TotalRLC_AM_BufferSize [enum=2]

maximumRLC_WindowSize: mws2047_MaximumRLC_WindowSize [enum=0]

maximumAM_EntityNumber: am6_MaximumAM_EntityNumberRLC_Cap [enum=3]

transportChannelCapability:

dl_TransChCapability:

maxNoBitsReceived: b5120_MaxNoBits [enum=4]

maxConvCodeBitsReceived: b1280_MaxNoBits [enum=1]

turboDecodingSupport:

supported: b5120_MaxNoBits [enum=4]

maxSimultaneousTransChs: e8_MaxSimultaneousTransChsDL [enum=1]

maxSimultaneousCCTrCH_Count: 1

maxReceivedTransportBlocks: tb16_MaxTransportBlocksDL [enum=2]

maxNumberOfTFC: tfc96_MaxNumberOfTFC_DL [enum=4]

maxNumberOfTF: tf64_MaxNumberOfTF [enum=1]

ul_TransChCapability:

maxNoBitsTransmitted: b3840_MaxNoBits [enum=3]

maxConvCodeBitsTransmitted: b1280_MaxNoBits [enum=1]

turboEncodingSupport:

supported: b3840_MaxNoBits [enum=3]

maxSimultaneousTransChs: e8_MaxSimultaneousTransChsUL [enum=2]

modeSpecificInfo:

fdd: NULL

maxTransmittedBlocks: tb8_MaxTransportBlocksUL [enum=2]

maxNumberOfTFC: tfc32_MaxNumberOfTFC_UL [enum=3]

maxNumberOfTF: tf32_MaxNumberOfTF [enum=0]

rf_Capability:

fddRF_Capability:

ue_PowerClass: 4

txRxFrequencySeparation: mhz190_TxRxFrequencySeparation [enum=0]

tddRF_Capability: Omitted

physicalChannelCapability:

fddPhysChCapability:

downlinkPhysChCapability:

maxNoDPCH_PDSCH_Codes: 3

maxNoPhysChBitsReceived: b9600_MaxNoPhysChBitsReceived [enum=6]

supportForSF_512: 0

supportOfPDSCH: 0

simultaneousSCCPCH_DPCH_Reception:

notSupported: NULL

uplinkPhysChCapability:

maxNoDPDCH_BitsTransmitted: b2400_MaxNoDPDCH_BitsTransmitted [enum=2]

supportOfPCPCH: 0

tddPhysChCapability: Omitted

ue_MultiModeRAT_Capability:

multiRAT_CapabilityList:

supportOfGSM: 0

supportOfMulticarrier: 0

multiModeCapability: fdd_MultiModeCapability [enum=1]

securityCapability:

cipheringAlgorithmCap: 0000000000000001

integrityProtectionAlgorithmCap: 0000000000000010

ue_positioning_Capability:

standaloneLocMethodsSupported: 0

ue_BasedOTDOA_Supported: 0

networkAssistedGPS_Supported: noNetworkAssistedGPS_NetworkAssistedGPS_Supported [enum=3]

supportForUE_GPS_TimingOfCellFrames: 0

supportForIPDL: 0

measurementCapability:

downlinkCompressedMode:

fdd_Measurements: 1

tdd_Measurements: Omitted

gsm_Measurements:

gsm900: 1

dcs1800: 1

gsm1900: 0

multiCarrierMeasurements: 0

uplinkCompressedMode:

fdd_Measurements: 1

tdd_Measurements: Omitted

gsm_Measurements:

gsm900: 1

dcs1800: 1

gsm1900: 0

multiCarrierMeasurements: 0

ue_RATSpecificCapability: Omitted

v370NonCriticalExtensions: Omitted

Layer 3 SDU:

[0]4A 0C 00 00 80 00 05 E2
[8]34 1A 20 90 98 CD 08 C5
[16]92 60 41 00 01 00 02 31
[24]F1 F0

#### RLC_AM_DATA_IND

LLA RRC @ 00:01:43.860

Channel ID: Rb2
Cell ID: -1

Message Details:

RLC_AM_DATA_IND:

cellId:-1

routingInfo:

rB_Identity:2

integrityResult:

integrityUsed (IntegrityStatus):i_pass

aM_message:

uL_DCCH_Message:

integrityCheckInfo: Omit

message: (UL_DCCH_MessageType)

rrcConnectionSetupComplete:

rrc_TransactionIdentifier:0

startList:

STARTSingle:

cn_DomainIdentity:ps_domain
start_Value:00000000000000000010

STARTSingle:

cn_DomainIdentity:cs_domain
start_Value:00000000000000000010

ue_RadioAccessCapability:

accessStratumReleaseIndicator:r99

pdcp_Capability:

losslessSRNS_RelocationSupport:true

supportForRfc2507:

supported (MaxHcContextSpace):by8192

rlc_Capability:

totalRLC_AM_BufferSize:kb50
maximumRLC_WindowSize:mws2047
maximumAM_EntityNumber (MaximumAM_EntityNumberRLC_Cap):am6

transportChannelCapability:

dl_TransChCapability:

maxNoBitsReceived (MaxNoBits):b5120
maxConvCodeBitsReceived (MaxNoBits):b1280

turboDecodingSupport: (TurboSupport)

supported (MaxNoBits):b5120

maxSimultaneousTransChs (MaxSimultaneousTransChsDL):e8
maxSimultaneousCCTrCH_Count:1
maxReceivedTransportBlocks (MaxTransportBlocksDL):tb16
maxNumberOfTFC (MaxNumberOfTFC_DL):tfc96
maxNumberOfTF:tf64

ul_TransChCapability:

maxNoBitsTransmitted (MaxNoBits):b3840
maxConvCodeBitsTransmitted (MaxNoBits):b1280

turboEncodingSupport: (TurboSupport)

supported (MaxNoBits):b3840

maxSimultaneousTransChs (MaxSimultaneousTransChsUL):e8

modeSpecificInfo:

fdd:

maxTransmittedBlocks (MaxTransportBlocksUL):tb8
maxNumberOfTFC (MaxNumberOfTFC_UL):tfc32
maxNumberOfTF:tf32

rf_Capability:

fddRF_Capability:

ue_PowerClass:4
txRxFrequencySeparation:mhz190

tddRF_Capability: Omit

physicalChannelCapability:

fddPhysChCapability:

downlinkPhysChCapability: (DL_PhysChCapabilityFDD)

maxNoDPCH_PDSCH_Codes:3
maxNoPhysChBitsReceived:b9600
supportForSF_512:false
supportOfPDSCH:false

simultaneousSCCPCH_DPCH_Reception:

notSupported:

uplinkPhysChCapability: (UL_PhysChCapabilityFDD)

maxNoDPDCH_BitsTransmitted:b2400
supportOfPCPCH:false

tddPhysChCapability: Omit

ue_MultiModeRAT_Capability:

multiRAT_CapabilityList: (MultiRAT_Capability)

supportOfGSM:false
supportOfMulticarrier:false

multiModeCapability:fdd

securityCapability:

cipheringAlgorithmCap:0000000000000001
integrityProtectionAlgorithmCap:0000000000000010

ue_positioning_Capability:

standaloneLocMethodsSupported:false
ue_BasedOTDOA_Supported:false
networkAssistedGPS_Supported:noNetworkAssistedGPS
supportForUE_GPS_TimingOfCellFrames:false
supportForIPDL:false

measurementCapability:

downlinkCompressedMode: (CompressedModeMeasCapability)

fdd_Measurements:true
tdd_Measurements: Omit

gsm_Measurements:

gsm900:true
dcs1800:true
gsm1900:false

multiCarrierMeasurements:false

uplinkCompressedMode: (CompressedModeMeasCapability)

fdd_Measurements:true
tdd_Measurements: Omit

gsm_Measurements:

gsm900:true
dcs1800:true
gsm1900:false

multiCarrierMeasurements:false

ue_RATSpecificCapability: (InterRAT_UE_RadioAccessCapabilityList) Omit

v370NonCriticalExtensions: Omit

#### PHY_DATA_IND

PHY MAC @ 00:01:43.880

BTS unit: 1:2
Channel No: 0 Name: U_RACH
CFN: 137

Message Details:

TFI:0
TB set size:168
TB size:168
TB set (raw):

[0]50 00 12 80 00 15 88 D1
[8]01 58 40 40 08 07 88 80
[16]00 08 08 50 A7 00

TB set (decoded):

TB 0:

TCTF:1
UEID type:C-RNTI
UEID:1
C/T:2
MAC SDU (144 bits):

[0]80 00 15 88 D1 01 58 40
[8]40 08 07 88 80 00 08 08
[16]50 A7

#### MAC_DATA_IND

MAC RLC @ 00:01:43.880

Category: Configuration
BTS unit: 1:2
Channel No: 3 Name: DCCH
CFN: 137

Message Details:

RLC PDU size (bits):142
RLC PDU (raw):

[0]80 00 15 88 D1 01 58 40
[8]40 08 07 88 80 00 08 08
[16]50 A7

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:0
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]15 88 D1 01 58 40 40 08
[8]07 88 80 00 08 08 50 A7

#### PHY_DATA_IND

PHY MAC @ 00:01:43.940

BTS unit: 1:2
Channel No: 0 Name: U_RACH
CFN: 143

Message Details:

TFI:0
TB set size:168
TB size:168
TB set (raw):

[0]50 00 12 80 08 9C 11 9A
[8]60 19 31 E5 03 00 CD 58
[16]91 A0 B8 B1 38 00

TB set (decoded):

TB 0:

TCTF:1
UEID type:C-RNTI
UEID:1
C/T:2
MAC SDU (144 bits):

[0]80 08 9C 11 9A 60 19 31
[8]E5 03 00 CD 58 91 A0 B8
[16]B1 38

#### MAC_DATA_IND

MAC RLC @ 00:01:43.940

Category: Configuration
BTS unit: 1:2
Channel No: 3 Name: DCCH
CFN: 143

Message Details:

RLC PDU size (bits):142
RLC PDU (raw):

[0]80 08 9C 11 9A 60 19 31
[8]E5 03 00 CD 58 91 A0 B8
[16]B1 38

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:1
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]9C 11 9A 60 19 31 E5 03
[8]00 CD 58 91 A0 B8 B1 38

#### PHY_DATA_IND

PHY MAC @ 00:01:44.000

BTS unit: 1:2
Channel No: 0 Name: U_RACH
CFN: 149

Message Details:

TFI:0
TB set size:168
TB size:168
TB set (raw):

[0]50 00 12 80 10 38 10 C0
[8]2F A0 91 A2 B3 C1 88 17
[16]2A 01 90 10 00 00

TB set (decoded):

TB 0:

TCTF:1
UEID type:C-RNTI
UEID:1
C/T:2
MAC SDU (144 bits):

[0]80 10 38 10 C0 2F A0 91
[8]A2 B3 C1 88 17 2A 01 90
[16]10 00

#### MAC_DATA_IND

MAC RLC @ 00:01:44.000

Category: Configuration
BTS unit: 1:2
Channel No: 3 Name: DCCH
CFN: 149

Message Details:

RLC PDU size (bits):142
RLC PDU (raw):

[0]80 10 38 10 C0 2F A0 91
[8]A2 B3 C1 88 17 2A 01 90
[16]10 00

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:2
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]38 10 C0 2F A0 91 A2 B3
[8]C1 88 17 2A 01 90 10 00

#### PHY_DATA_IND

PHY MAC @ 00:01:44.060

BTS unit: 1:2
Channel No: 0 Name: U_RACH
CFN: 155

Message Details:

TFI:0
TB set size:168
TB size:168
TB set (raw):

[0]50 00 12 80 1D 09 FE 02
[8]00 00 40 55 55 55 55 55
[16]55 55 55 55 55 00

TB set (decoded):

TB 0:

TCTF:1
UEID type:C-RNTI
UEID:1
C/T:2
MAC SDU (144 bits):

[0]80 1D 09 FE 02 00 00 40
[8]55 55 55 55 55 55 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:01:44.060

Category: Configuration
BTS unit: 1:2
Channel No: 3 Name: DCCH
CFN: 155

Message Details:

RLC PDU size (bits):142
RLC PDU (raw):

[0]80 1D 09 FE 02 00 00 40
[8]55 55 55 55 55 55 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:3
Polling bit:1 (request a status report)
Length indicator 0 (octets):4
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (4 octets):

[0]02 00 00 40
Padding associated with length indicator 1 (10 octets):

[0]55 55 55 55 55 55 55 55
[8]55 55

#### RLC_AM_DATA_IND: initialDirectTransfer

RLC RRC @ 00:01:44.070

Channel No: 3 Name: DCCH

Message Details:

UL_DCCH_Message:

integrityCheckInfo: Omitted

message:

initialDirectTransfer:

cn_DomainIdentity: ps_domain_CN_DomainIdentity [enum=1]

intraDomainNasNodeSelector:

version:

release99:

cn_Type:

gsm_Map_IDNNS:

routingbasis:

tMSIofdifferentPLMN:

routingparameter: 0011010001

enteredparameter: 0

nas_Message: 08080100F1100001010A14F382334C03263CA06019AB123417162707021805F4123456783102E54032020000

measuredResultsOnRACH: Omitted

v3a0NonCriticalExtensions:

initialDirectTransfer_v3a0ext:

start_Value: 00000000000000000010

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]15 88 D1 01 58 40 40 08
[8]07 88 80 00 08 08 50 A7
[16]9C 11 9A 60 19 31 E5 03
[24]00 CD 58 91 A0 B8 B1 38
[32]38 10 C0 2F A0 91 A2 B3
[40]C1 88 17 2A 01 90 10 00
[48]02 00 00 40

#### RRC_DATA_IND: gmm:routingAreaUpdateRequest

RRC NAS @ 00:01:44.070

Cell ID: -1

Message Details:

ROUTINGAREAUPDATEREQUEST:

skipIndicator: 0000

gMMProtocolDiscriminator: 1000

msgType: 00001000

gprsCiphKeySeqNo:

spare1: 0

keySeq: 000

updateType:

for: 0

value: 001

oldRAI:

plmn: 00F110

lac: 0001

rac: 01

msRadioAccessCap:

iel: 0A

value: 14F382334C03263CA060

oldPTMSI_Signature:

iei: 00011001

value: AB1234

readyTimer:

iei: 00010111

unit: 000

value: 10110

drxParameter:

iei: 00100111

splitPGcycleCode: 00000111

cnDRXcoef: 0000

splitOnCCCH: 0

nonDRXtimer: 010

tmsiStatus: Omitted

ptmsi:

iei: 00011000

iel: 05

iDigit1: 1111

oddEvenInd: 0

typeOfId: 100

otherDigits: 12345678

msnetworkcap:

iei: 00110001

iel: 02

value: E540

pDP_ContextStatus:

iei: 00110010

iel: 02

nSAPI: 0000000000000000

#### MAC_DATA_REQ

RLC MAC @ 00:01:44.070

Category: Configuration
BTS unit: 1:2
Channel No: 3 Name: DCCH
CFN: 176

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 40 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:4

#### PHY_DATA_REQ

MAC PHY @ 00:01:44.070

BTS unit: 1:2
Channel No: 0 Name: FACH
CFN: 176

Message Details:

TFI:1
TB set size:168
TB size:168
TB set (raw):

[0]D0 00 12 02 00 40 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00 00 00

TB set (decoded):

TB 0:

TCTF:3
UEID type:C-RNTI
UEID:1
C/T:2
MAC SDU (144 bits):

[0]02 00 40 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### RRC_DATA_REQ: gmm:authenticationAndCipheringRequest

NAS RRC @ 00:01:44.110

Cell ID: -1

Message Details:

AUTHENTICATIONANDCIPHERINGREQUEST:

skipIndicator: 0000

gMMProtocolDiscriminator: 1000

msgType: 00010010

imeisvReq:

spare1: 0

value: 000

ciphAlgorithm:

spare1: 0

algorithm: 001

acRefNo:

value: 0011

forceToStandby:

spare: 0

value: 000

authRand:

iei: 00100001

randValue: 01010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101

gprsCiphKeySeqNo:

iei: 1000

spare1: 0

keySeq: 001

aUTN:

iei: 00101000

iel: 10

aUTN: 01100110000100010000000000110011001000101101110100000000000000000101010101000100011101110110011000010001000000000011001100100010

#### RLC_AM_DATA_REQ:downlinkDirectTransfer

RRC RLC @ 00:01:44.110

Channel No: 3 Name: DCCH

Message Details:

Opt1: 0

Opt2: 0

DL_DCCH_Message:

integrityCheckInfo: Omitted

message:

downlinkDirectTransfer:

r3:

downlinkDirectTransfer_r3:

rrc_TransactionIdentifier: 0

cn_DomainIdentity: ps_domain_CN_DomainIdentity [enum=1]

nas_Message: 0812013021555555555555555555555555555555558128106611003322DD00005544776611003322

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]14 20 4E 10 24 02 60 42
[8]AA AA AA AA AA AA AA AA
[16]AA AA AA AA AA AA AA AB
[24]02 50 20 CC 22 00 66 45
[32]BA 00 00 AA 88 EE CC 22
[40]00 66 44

#### MAC_DATA_REQ

RLC MAC @ 00:01:44.120

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 181

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 00 14 20 4E 10 24 02
[8]60 42 AA AA AA AA AA AA
[16]AA AA

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:0
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]14 20 4E 10 24 02 60 42
[8]AA AA AA AA AA AA AA AA

#### MAC_DATA_REQ

RLC MAC @ 00:01:44.120

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 181

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 08 AA AA AA AA AA AA
[8]AA AB 02 50 20 CC 22 00
[16]66 45

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:1
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]AA AA AA AA AA AA AA AB
[8]02 50 20 CC 22 00 66 45

#### MAC_DATA_REQ

RLC MAC @ 00:01:44.120

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 181

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 15 17 FE BA 00 00 AA
[8]88 EE CC 22 00 66 44 00
[16]00 00

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:2
Polling bit:1 (request a status report)
Length indicator 0 (octets):11
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (11 octets):

[0]BA 00 00 AA 88 EE CC 22
[8]00 66 44
Padding associated with length indicator 1 (3 octets):

[0]00 00 00

#### PHY_DATA_REQ

MAC PHY @ 00:01:44.120

BTS unit: 1:2
Channel No: 0 Name: FACH
CFN: 181

Message Details:

TFI:2
TB set size:336
TB size:168
TB set (raw, each TB word aligned):

[0]D0 00 12 80 00 14 20 4E
[8]10 24 02 60 42 AA AA AA
[16]AA AA AA AA AA 00 D0 00
[24]12 80 08 AA AA AA AA AA
[32]AA AA AB 02 50 20 CC 22
[40]00 66 45 00

TB set (decoded):

TB 0:

TCTF:3
UEID type:C-RNTI
UEID:1
C/T:2
MAC SDU (144 bits):

[0]80 00 14 20 4E 10 24 02
[8]60 42 AA AA AA AA AA AA
[16]AA AA

TB 1:

TCTF:3
UEID type:C-RNTI
UEID:1
C/T:2
MAC SDU (144 bits):

[0]80 08 AA AA AA AA AA AA
[8]AA AB 02 50 20 CC 22 00
[16]66 45

#### PHY_DATA_REQ

MAC PHY @ 00:01:44.130

BTS unit: 1:2
Channel No: 0 Name: FACH
CFN: 182

Message Details:

TFI:1
TB set size:168
TB size:168
TB set (raw):

[0]D0 00 12 80 15 17 FE BA
[8]00 00 AA 88 EE CC 22 00
[16]66 44 00 00 00 00

TB set (decoded):

TB 0:

TCTF:3
UEID type:C-RNTI
UEID:1
C/T:2
MAC SDU (144 bits):

[0]80 15 17 FE BA 00 00 AA
[8]88 EE CC 22 00 66 44 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:01:44.380

BTS unit: 1:2
Channel No: 0 Name: U_RACH
CFN: 187

Message Details:

TFI:0
TB set size:168
TB size:168
TB set (raw):

[0]50 00 12 02 00 30 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00 00 00

TB set (decoded):

TB 0:

TCTF:1
UEID type:C-RNTI
UEID:1
C/T:2
MAC SDU (144 bits):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### MAC_DATA_IND

MAC RLC @ 00:01:44.380

Category: Configuration
BTS unit: 1:2
Channel No: 3 Name: DCCH
CFN: 187

Message Details:

RLC PDU size (bits):142
RLC PDU (raw):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:3

#### PHY_DATA_IND

PHY MAC @ 00:01:44.550

BTS unit: 1:2
Channel No: 0 Name: U_RACH
CFN: 204

Message Details:

TFI:0
TB set size:168
TB size:168
TB set (raw):

[0]50 00 12 80 20 6C 80 A8
[8]40 98 19 12 AA 23 BB 31
[16]48 60 88 01 99 00

TB set (decoded):

TB 0:

TCTF:1
UEID type:C-RNTI
UEID:1
C/T:2
MAC SDU (144 bits):

[0]80 20 6C 80 A8 40 98 19
[8]12 AA 23 BB 31 48 60 88
[16]01 99

#### MAC_DATA_IND

MAC RLC @ 00:01:44.550

Category: Configuration
BTS unit: 1:2
Channel No: 3 Name: DCCH
CFN: 204

Message Details:

RLC PDU size (bits):142
RLC PDU (raw):

[0]80 20 6C 80 A8 40 98 19
[8]12 AA 23 BB 31 48 60 88
[16]01 99

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:4
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]6C 80 A8 40 98 19 12 AA
[8]23 BB 31 48 60 88 01 99

#### PHY_DATA_IND

PHY MAC @ 00:01:44.620

BTS unit: 1:2
Channel No: 0 Name: U_RACH
CFN: 211

Message Details:

TFI:0
TB set size:168
TB size:168
TB set (raw):

[0]50 00 12 80 2D 13 FE 16
[8]EE 67 FF 74 CC 45 DD 50
[16]55 55 55 55 55 00

TB set (decoded):

TB 0:

TCTF:1
UEID type:C-RNTI
UEID:1
C/T:2
MAC SDU (144 bits):

[0]80 2D 13 FE 16 EE 67 FF
[8]74 CC 45 DD 50 55 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:01:44.620

Category: Configuration
BTS unit: 1:2
Channel No: 3 Name: DCCH
CFN: 211

Message Details:

RLC PDU size (bits):142
RLC PDU (raw):

[0]80 2D 13 FE 16 EE 67 FF
[8]74 CC 45 DD 50 55 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:5
Polling bit:1 (request a status report)
Length indicator 0 (octets):9
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (9 octets):

[0]16 EE 67 FF 74 CC 45 DD
[8]50
Padding associated with length indicator 1 (5 octets):

[0]55 55 55 55 55

#### RLC_AM_DATA_IND: uplinkDirectTransfer

RLC RRC @ 00:01:44.630

Channel No: 3 Name: DCCH

Message Details:

UL_DCCH_Message:

integrityCheckInfo: Omitted

message:

uplinkDirectTransfer:

cn_DomainIdentity: ps_domain_CN_DomainIdentity [enum=1]

nas_Message: 0813032255447766290C11003322DDCCFFEE9988BBAA

measuredResultsOnRACH: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]6C 80 A8 40 98 19 12 AA
[8]23 BB 31 48 60 88 01 99
[16]16 EE 67 FF 74 CC 45 DD
[24]50

#### RRC_DATA_IND: gmm:authenticationAndCipheringResponse

RRC NAS @ 00:01:44.630

Cell ID: -1

Message Details:

AUTHENTICATIONANDCIPHERINGRESPONSE:

skipIndicator: 0000

gMMProtocolDiscriminator: 1000

msgType: 00010011

spare4: 0000

acRefNo:

value: 0011

authRsp:

iei: 00100010

value: 01010101010001000111011101100110

imeisv: Omitted

authRspExt:

iei: 00101001

iel: 0C

rES: 000100010000000000110011001000101101110111001100111111111110111010011001100010001011101110101010

#### MAC_DATA_REQ

RLC MAC @ 00:01:44.630

Category: Configuration
BTS unit: 1:2
Channel No: 3 Name: DCCH
CFN: 232

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 60 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:6

#### PHY_DATA_REQ

MAC PHY @ 00:01:44.630

BTS unit: 1:2
Channel No: 0 Name: FACH
CFN: 232

Message Details:

TFI:1
TB set size:168
TB size:168
TB set (raw):

[0]D0 00 12 02 00 60 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00 00 00

TB set (decoded):

TB 0:

TCTF:3
UEID type:C-RNTI
UEID:1
C/T:2
MAC SDU (144 bits):

[0]02 00 60 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### CRLC_SecurityMode_Config_REQ

RRC LLA @ 00:01:44.650

Cell ID: -1

Message Details:

CRLC_SecurityMode_Config_REQ:

cellId:-1

rlcSecurityInfo: (SecurityInfo)

cn_DomainIdentity:ps_domain
startValue (START_Value):00000000000000000000
cipheringKey:01000100011101110110011000010001000000000011001100100010110111011100110011111111111011101001100110001000101110111010101001010101
integrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
gsmCipheringKey: Omit

#### CRLC_SecurityMode_Config_REQ

RRC RLC @ 00:01:44.650

Message Details:

cellIdentity: 1

rlcSecurityInfo:

cn_DomainIdentity: ps_domain_CN_DomainIdentity

startValue: 00000000000000000000

cipheringKey: 01000100011101110110011000010001000000000011001100100010110111011100110011111111111011101001100110001000101110111010101001010101

integrityKey: 01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100

#### CRLC_SecurityMode_Config_CNF

LLA RRC @ 00:01:44.670

Cell ID: -1

Message Details:

CRLC_SecurityMode_Config_CNF:

cellId:-1

#### CRLC_SetRRC_MessageSN_REQ

RRC LLA @ 00:01:44.670

Channel ID: Rb0
Cell ID: 6

Message Details:

CRLC_SetRRC_MessageSN_REQ:

cellId:6

routingInfo:

rB_Identity:0

count_I_LSB_UL (RRC_SequenceNumber): Omit
count_I_LSB_DL (RRC_SequenceNumber):0

#### CRLC_SetRRC_MessageSN_CNF

LLA RRC @ 00:01:44.690

Channel ID: Rb0
Cell ID: 6

Message Details:

CRLC_SetRRC_MessageSN_CNF:

cellId:6

routingInfo:

rB_Identity:0

#### CRLC_SetRRC_MessageSN_REQ

RRC LLA @ 00:01:44.690

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_REQ:

cellId:-1

routingInfo:

rB_Identity:1

count_I_LSB_UL (RRC_SequenceNumber): Omit
count_I_LSB_DL (RRC_SequenceNumber):0

#### CRLC_SetRRC_MessageSN_CNF

LLA RRC @ 00:01:44.700

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_CNF:

cellId:-1

routingInfo:

rB_Identity:1

#### CRLC_SetRRC_MessageSN_REQ

RRC LLA @ 00:01:44.700

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_REQ:

cellId:-1

routingInfo:

rB_Identity:2

count_I_LSB_UL (RRC_SequenceNumber): Omit
count_I_LSB_DL (RRC_SequenceNumber):0

#### CRLC_SetRRC_MessageSN_CNF

LLA RRC @ 00:01:44.720

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_CNF:

cellId:-1

routingInfo:

rB_Identity:2

#### CRLC_SetRRC_MessageSN_REQ

RRC LLA @ 00:01:44.720

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_REQ:

cellId:-1

routingInfo:

rB_Identity:3

count_I_LSB_UL (RRC_SequenceNumber): Omit
count_I_LSB_DL (RRC_SequenceNumber):0

#### CRLC_SetRRC_MessageSN_CNF

LLA RRC @ 00:01:44.730

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_CNF:

cellId:-1

routingInfo:

rB_Identity:3

#### CRLC_SetRRC_MessageSN_REQ

RRC LLA @ 00:01:44.730

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_REQ:

cellId:-1

routingInfo:

rB_Identity:4

count_I_LSB_UL (RRC_SequenceNumber): Omit
count_I_LSB_DL (RRC_SequenceNumber):0

#### CRLC_SetRRC_MessageSN_CNF

LLA RRC @ 00:01:44.750

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_CNF:

cellId:-1

routingInfo:

rB_Identity:4

#### CRLC_Integrity_Activate_REQ

RRC LLA @ 00:01:44.750

Cell ID: -1

Message Details:

CRLC_Integrity_Activate_REQ:

cellId:-1
cn_DomainIdentity:ps_domain

integrityActivationInfo:

integrityProtectionModeInfo:

integrityProtectionModeCommand:

startIntegrityProtection:

integrityProtInitNumber:00001111000011110000111100001111

integrityProtectionAlgorithm:uia1

#### CRLC_Integrity_Activate_REQ

RRC RLC @ 00:01:44.750

Message Details:

cellIdentity: 1

integrityActivationInfo:

integrityProtectionModeInfo:

integrityProtectionModeCommand:

startIntegrityProtection:

integrityProtInitNumber: 00001111000011110000111100001111

#### CRLC_Integrity_Activate_CNF

LLA RRC @ 00:01:44.760

Cell ID: -1

Message Details:

CRLC_Integrity_Activate_CNF:

cellId:-1

#### CRLC_SequenceNumber_REQ

RRC LLA @ 00:01:44.760

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_SequenceNumber_REQ:

cellId:-1

routingInfo:

rB_Identity:1

#### CRLC Sequence Number CNF

RLC RRC @ 00:01:44.780

BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 247

Message Details:

Sequence Number Results:

DL Count C:00000000000000000000000000000000
UL Count C:00000000000000000000000000000000

#### CRLC_SequenceNumber_CNF

LLA RRC @ 00:01:44.780

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_SequenceNumber_CNF:

cellId:-1

routingInfo:

rB_Identity:1

count_C_MSB_UL (COUNT_C_MSB):0
count_C_LSB_UL (RLC_SequenceNumber):0
count_C_MSB_DL (COUNT_C_MSB):0
count_C_LSB_DL (RLC_SequenceNumber):0

#### CRLC_SequenceNumber_REQ

RRC LLA @ 00:01:44.780

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_SequenceNumber_REQ:

cellId:-1

routingInfo:

rB_Identity:2

#### CRLC Sequence Number CNF

RLC RRC @ 00:01:44.800

BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 249

Message Details:

Sequence Number Results:

DL Count C:00000000000000000000000000000000
UL Count C:00000000000000000000000000000010

#### CRLC_SequenceNumber_CNF

LLA RRC @ 00:01:44.810

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_SequenceNumber_CNF:

cellId:-1

routingInfo:

rB_Identity:2

count_C_MSB_UL (COUNT_C_MSB):0
count_C_LSB_UL (RLC_SequenceNumber):2
count_C_MSB_DL (COUNT_C_MSB):0
count_C_LSB_DL (RLC_SequenceNumber):0

#### CRLC_SequenceNumber_REQ

RRC LLA @ 00:01:44.810

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_SequenceNumber_REQ:

cellId:-1

routingInfo:

rB_Identity:3

#### CRLC Sequence Number CNF

RLC RRC @ 00:01:44.830

BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 252

Message Details:

Sequence Number Results:

DL Count C:00000000000000000000000000000011
UL Count C:00000000000000000000000000000110

#### CRLC_SequenceNumber_CNF

LLA RRC @ 00:01:44.830

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_SequenceNumber_CNF:

cellId:-1

routingInfo:

rB_Identity:3

count_C_MSB_UL (COUNT_C_MSB):0
count_C_LSB_UL (RLC_SequenceNumber):6
count_C_MSB_DL (COUNT_C_MSB):0
count_C_LSB_DL (RLC_SequenceNumber):3

#### CRLC_SequenceNumber_REQ

RRC LLA @ 00:01:44.830

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_SequenceNumber_REQ:

cellId:-1

routingInfo:

rB_Identity:4

#### CRLC Sequence Number CNF

RLC RRC @ 00:01:44.840

BTS unit: 1:1
Channel No: 4 Name: DCCH
CFN: 253

Message Details:

Sequence Number Results:

DL Count C:00000000000000000000000000000000
UL Count C:00000000000000000000000000000000

#### CRLC_SequenceNumber_CNF

LLA RRC @ 00:01:44.840

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_SequenceNumber_CNF:

cellId:-1

routingInfo:

rB_Identity:4

count_C_MSB_UL (COUNT_C_MSB):0
count_C_LSB_UL (RLC_SequenceNumber):0
count_C_MSB_DL (COUNT_C_MSB):0
count_C_LSB_DL (RLC_SequenceNumber):0

#### CRLC_Suspend_REQ

RRC LLA @ 00:01:44.840

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Suspend_REQ:

cellId:-1

routingInfo:

rB_Identity:1

n (RLC_SequenceNumber):0

#### CRLC Suspend REQ

LLA RLC @ 00:01:44.850

BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 254

Message Details:

N:0

#### CRLC Suspend CNF

RLC LLA @ 00:01:44.850

BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 254

Message Details:

Sequence Number:0

#### CRLC_Suspend_CNF

LLA RRC @ 00:01:44.860

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Suspend_CNF:

cellId:-1

routingInfo:

rB_Identity:1

vt (RLC_SequenceNumber):0

#### CRLC_Suspend_REQ

RRC LLA @ 00:01:44.860

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Suspend_REQ:

cellId:-1

routingInfo:

rB_Identity:3

n (RLC_SequenceNumber):3

#### CRLC_Suspend_CNF

LLA RRC @ 00:01:44.870

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Suspend_CNF:

cellId:-1

routingInfo:

rB_Identity:3

vt (RLC_SequenceNumber):3

#### CRLC_Suspend_REQ

RRC LLA @ 00:01:44.870

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Suspend_REQ:

cellId:-1

routingInfo:

rB_Identity:4

n (RLC_SequenceNumber):0

#### CRLC Suspend REQ

LLA RLC @ 00:01:44.870

BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 0

Message Details:

N:3

#### CRLC Suspend CNF

RLC LLA @ 00:01:44.870

BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 0

Message Details:

Sequence Number:3

#### CRLC Suspend REQ

LLA RLC @ 00:01:44.880

BTS unit: 1:1
Channel No: 4 Name: DCCH
CFN: 1

Message Details:

N:0

#### CRLC Suspend CNF

RLC LLA @ 00:01:44.880

BTS unit: 1:1
Channel No: 4 Name: DCCH
CFN: 1

Message Details:

Sequence Number:0

#### CRLC_Suspend_CNF

LLA RRC @ 00:01:44.890

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Suspend_CNF:

cellId:-1

routingInfo:

rB_Identity:4

vt (RLC_SequenceNumber):0

#### CRLC_Ciphering_Activate_REQ

RRC LLA @ 00:01:44.890

Cell ID: -1

Message Details:

CRLC_Ciphering_Activate_REQ:

cellId:-1
ratType:fdd
cn_DomainIdentity:ps_domain

ciphActivationInfo:

cipheringModeInfo:

cipheringModeCommand:

startRestart (CipheringAlgorithm):uea0

activationTimeForDPCH (ActivationTime): Omit

rb_DL_CiphActivationTimeInfo: (RB_ActivationTimeInfoList)

RB_ActivationTimeInfo:

rb_Identity:1
rlc_SequenceNumber:0

incHFN (RLC_IncMode):notInc

#### CRLC_Ciphering_Activate_CNF

LLA RRC @ 00:01:44.900

Cell ID: -1

Message Details:

CRLC_Ciphering_Activate_CNF:

cellId:-1

#### CRLC_Ciphering_Activate_REQ

RRC LLA @ 00:01:44.900

Cell ID: -1

Message Details:

CRLC_Ciphering_Activate_REQ:

cellId:-1
ratType:fdd
cn_DomainIdentity:ps_domain

ciphActivationInfo:

cipheringModeInfo:

cipheringModeCommand:

startRestart (CipheringAlgorithm):uea0

activationTimeForDPCH (ActivationTime): Omit

rb_DL_CiphActivationTimeInfo: (RB_ActivationTimeInfoList)

RB_ActivationTimeInfo:

rb_Identity:2
rlc_SequenceNumber:2

incHFN (RLC_IncMode):notInc

#### CRLC_Ciphering_Activate_CNF

LLA RRC @ 00:01:44.920

Cell ID: -1

Message Details:

CRLC_Ciphering_Activate_CNF:

cellId:-1

#### CRLC_Ciphering_Activate_REQ

RRC LLA @ 00:01:44.920

Cell ID: -1

Message Details:

CRLC_Ciphering_Activate_REQ:

cellId:-1
ratType:fdd
cn_DomainIdentity:ps_domain

ciphActivationInfo:

cipheringModeInfo:

cipheringModeCommand:

startRestart (CipheringAlgorithm):uea0

activationTimeForDPCH (ActivationTime): Omit

rb_DL_CiphActivationTimeInfo: (RB_ActivationTimeInfoList)

RB_ActivationTimeInfo:

rb_Identity:3
rlc_SequenceNumber:3

incHFN (RLC_IncMode):notInc

#### CRLC_Ciphering_Activate_CNF

LLA RRC @ 00:01:44.940

Cell ID: -1

Message Details:

CRLC_Ciphering_Activate_CNF:

cellId:-1

#### CRLC_Ciphering_Activate_REQ

RRC LLA @ 00:01:44.940

Cell ID: -1

Message Details:

CRLC_Ciphering_Activate_REQ:

cellId:-1
ratType:fdd
cn_DomainIdentity:ps_domain

ciphActivationInfo:

cipheringModeInfo:

cipheringModeCommand:

startRestart (CipheringAlgorithm):uea0

activationTimeForDPCH (ActivationTime): Omit

rb_DL_CiphActivationTimeInfo: (RB_ActivationTimeInfoList)

RB_ActivationTimeInfo:

rb_Identity:4
rlc_SequenceNumber:0

incHFN (RLC_IncMode):notInc

#### CRLC_Ciphering_Activate_CNF

LLA RRC @ 00:01:44.950

Cell ID: -1

Message Details:

CRLC_Ciphering_Activate_CNF:

cellId:-1

#### CRLC_Integrity_Activate_REQ

RRC LLA @ 00:01:44.950

Cell ID: -1

Message Details:

CRLC_Integrity_Activate_REQ:

cellId:-1
cn_DomainIdentity:ps_domain

integrityActivationInfo:

ul_IntegProtActivationInfo: (IntegrityProtActivationInfoList)

SS_IntegrityProtActivationTimeInfo:

rb_Identity:2
rrc_MessageSequenceNumber:0

#### CMAC Integrity Check Request

RRC MAC @ 00:01:44.970

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000001
Data:

[0]00 00 00 01
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:1 (RNC to UE)
Message Length (bits):200
Message:

[0]80 00 00 01 04 0C 00 00
[8]80 01 20 C0 00 01 00 21
[16]00 18 C0 02 0F 0F 0F 0F
[24]80

#### CMAC Integrity Check Result

MAC RRC @ 00:01:44.970

Message Details:

Integrity Check Result:

MAC-I:01110001101111100101001001010100
Data:

[0]71 BE 52 54

#### CRLC_Integrity_Activate_CNF

LLA RRC @ 00:01:44.970

Cell ID: -1

Message Details:

CRLC_Integrity_Activate_CNF:

cellId:-1

#### RLC_AM_DATA_REQ

RRC LLA @ 00:01:44.970

Channel ID: Rb2
Cell ID: -1

Message Details:

RLC_AM_DATA_REQ:

cellId:-1

routingInfo:

rB_Identity:2

confirmationRequest: (AmConfirmationRequest)

noConfirmationRequest:

aM_message:

dL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode:00000000000000000000000000000000
rrc_MessageSequenceNumber:0

message: (DL_DCCH_MessageType)

securityModeCommand:

r3:

securityModeCommand_r3: (SecurityModeCommand_r3_IEs)

rrc_TransactionIdentifier:0

securityCapability:

cipheringAlgorithmCap:0000000000000001
integrityProtectionAlgorithmCap:0000000000000010

cipheringModeInfo:

cipheringModeCommand:

startRestart (CipheringAlgorithm):uea0

activationTimeForDPCH (ActivationTime): Omit

rb_DL_CiphActivationTimeInfo: (RB_ActivationTimeInfoList)

RB_ActivationTimeInfo:

rb_Identity:1
rlc_SequenceNumber:0

RB_ActivationTimeInfo:

rb_Identity:2
rlc_SequenceNumber:2

RB_ActivationTimeInfo:

rb_Identity:3
rlc_SequenceNumber:3

RB_ActivationTimeInfo:

rb_Identity:4
rlc_SequenceNumber:0

integrityProtectionModeInfo:

integrityProtectionModeCommand:

startIntegrityProtection:

integrityProtInitNumber:00001111000011110000111100001111

integrityProtectionAlgorithm:uia1

cn_DomainIdentity:ps_domain

ue_SystemSpecificSecurityCap: (InterRAT_UE_SecurityCapList) Omit

laterNonCriticalExtensions: Omit

#### RLC_AM_DATA_REQ: securityModeCommand

LLA RLC @ 00:01:44.970

Channel No: 2 Name: DCCH

Message Details:

DL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode: 01110001101111100101001001010100

rrc_MessageSequenceNumber: 1

message:

securityModeCommand:

r3:

securityModeCommand_r3:

rrc_TransactionIdentifier: 0

securityCapability:

cipheringAlgorithmCap: 0000000000000001

integrityProtectionAlgorithmCap: 0000000000000010

cipheringModeInfo:

cipheringModeCommand:

startRestart: uea0_CipheringAlgorithm [enum=0]

activationTimeForDPCH: Omitted

rb_DL_CiphActivationTimeInfo:

RB_ActivationTimeInfoList.element:

rb_Identity: 1

rlc_SequenceNumber: 0

RB_ActivationTimeInfoList.element:

rb_Identity: 2

rlc_SequenceNumber: 2

RB_ActivationTimeInfoList.element:

rb_Identity: 3

rlc_SequenceNumber: 3

RB_ActivationTimeInfoList.element:

rb_Identity: 4

rlc_SequenceNumber: 0

integrityProtectionModeInfo:

integrityProtectionModeCommand:

startIntegrityProtection:

integrityProtInitNumber: 00001111000011110000111100001111

integrityProtectionAlgorithm: uia1_IntegrityProtectionAlgorithm [enum=0]

cn_DomainIdentity: ps_domain_CN_DomainIdentity [enum=1]

ue_SystemSpecificSecurityCap: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]B8 DF 29 2A 0C 0C 00 00
[8]80 01 20 C0 00 01 00 21
[16]00 18 C0 02 0F 0F 0F 0F
[24]80

#### MAC_DATA_REQ

RLC MAC @ 00:01:44.980

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 11

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 00 B8 DF 29 2A 0C 0C
[8]00 00 80 01 20 C0 00 01
[16]00 21

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:0
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]B8 DF 29 2A 0C 0C 00 00
[8]80 01 20 C0 00 01 00 21

#### MAC_DATA_REQ

RLC MAC @ 00:01:44.980

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 11

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 0D 13 FE 00 18 C0 02
[8]0F 0F 0F 0F 80 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:1
Polling bit:1 (request a status report)
Length indicator 0 (octets):9
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (9 octets):

[0]00 18 C0 02 0F 0F 0F 0F
[8]80
Padding associated with length indicator 1 (5 octets):

[0]00 00 00 00 00

#### PHY_DATA_REQ

MAC PHY @ 00:01:44.990

BTS unit: 1:2
Channel No: 0 Name: FACH
CFN: 12

Message Details:

TFI:2
TB set size:336
TB size:168
TB set (raw, each TB word aligned):

[0]D0 00 11 80 00 B8 DF 29
[8]2A 0C 0C 00 00 80 01 20
[16]C0 00 01 00 21 00 D0 00
[24]11 80 0D 13 FE 00 18 C0
[32]02 0F 0F 0F 0F 80 00 00
[40]00 00 00 00

TB set (decoded):

TB 0:

TCTF:3
UEID type:C-RNTI
UEID:1
C/T:1
MAC SDU (144 bits):

[0]80 00 B8 DF 29 2A 0C 0C
[8]00 00 80 01 20 C0 00 01
[16]00 21

TB 1:

TCTF:3
UEID type:C-RNTI
UEID:1
C/T:1
MAC SDU (144 bits):

[0]80 0D 13 FE 00 18 C0 02
[8]0F 0F 0F 0F 80 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:01:45.240

BTS unit: 1:2
Channel No: 0 Name: U_RACH
CFN: 17

Message Details:

TFI:0
TB set size:168
TB size:168
TB set (raw):

[0]50 00 11 02 00 20 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00 00 00

TB set (decoded):

TB 0:

TCTF:1
UEID type:C-RNTI
UEID:1
C/T:1
MAC SDU (144 bits):

[0]02 00 20 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### MAC_DATA_IND

MAC RLC @ 00:01:45.240

Category: Configuration
BTS unit: 1:2
Channel No: 2 Name: DCCH
CFN: 17

Message Details:

RLC PDU size (bits):142
RLC PDU (raw):

[0]02 00 20 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:2

#### PHY_DATA_IND

PHY MAC @ 00:01:45.320

BTS unit: 1:2
Channel No: 0 Name: U_RACH
CFN: 25

Message Details:

TFI:0
TB set size:168
TB size:168
TB set (raw):

[0]50 00 11 80 10 FE 6E 85
[8]3F 0D 31 00 00 01 80 00
[16]02 00 E2 00 61 00

TB set (decoded):

TB 0:

TCTF:1
UEID type:C-RNTI
UEID:1
C/T:1
MAC SDU (144 bits):

[0]80 10 FE 6E 85 3F 0D 31
[8]00 00 01 80 00 02 00 E2
[16]00 61

#### MAC_DATA_IND

MAC RLC @ 00:01:45.320

Category: Configuration
BTS unit: 1:2
Channel No: 2 Name: DCCH
CFN: 25

Message Details:

RLC PDU size (bits):142
RLC PDU (raw):

[0]80 10 FE 6E 85 3F 0D 31
[8]00 00 01 80 00 02 00 E2
[16]00 61

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:2
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]FE 6E 85 3F 0D 31 00 00
[8]01 80 00 02 00 E2 00 61

#### PHY_DATA_IND

PHY MAC @ 00:01:45.420

BTS unit: 1:2
Channel No: 0 Name: U_RACH
CFN: 35

Message Details:

TFI:0
TB set size:168
TB size:168
TB set (raw):

[0]50 00 11 80 1D 05 FE 80
[8]00 55 55 55 55 55 55 55
[16]55 55 55 55 55 00

TB set (decoded):

TB 0:

TCTF:1
UEID type:C-RNTI
UEID:1
C/T:1
MAC SDU (144 bits):

[0]80 1D 05 FE 80 00 55 55
[8]55 55 55 55 55 55 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:01:45.420

Category: Configuration
BTS unit: 1:2
Channel No: 2 Name: DCCH
CFN: 35

Message Details:

RLC PDU size (bits):142
RLC PDU (raw):

[0]80 1D 05 FE 80 00 55 55
[8]55 55 55 55 55 55 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:3
Polling bit:1 (request a status report)
Length indicator 0 (octets):2
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (2 octets):

[0]80 00
Padding associated with length indicator 1 (12 octets):

[0]55 55 55 55 55 55 55 55
[8]55 55 55 55

#### MAC_DATA_REQ

RLC MAC @ 00:01:45.430

Category: Configuration
BTS unit: 1:2
Channel No: 2 Name: DCCH
CFN: 56

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 40 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:4

#### PHY_DATA_REQ

MAC PHY @ 00:01:45.430

BTS unit: 1:2
Channel No: 0 Name: FACH
CFN: 56

Message Details:

TFI:1
TB set size:168
TB size:168
TB set (raw):

[0]D0 00 11 02 00 40 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00 00 00

TB set (decoded):

TB 0:

TCTF:3
UEID type:C-RNTI
UEID:1
C/T:1
MAC SDU (144 bits):

[0]02 00 40 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### CMAC Integrity Check Request

RRC MAC @ 00:01:45.450

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000001
Data:

[0]00 00 00 01
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:0 (UE to RNC)
Message Length (bits):144
Message:

[0]80 00 00 01 05 31 00 00
[8]01 80 00 02 00 E2 00 61
[16]80 00

#### RLC_AM_DATA_IND: securityModeComplete

RLC LLA @ 00:01:45.450

Channel No: 2 Name: DCCH

Message Details:

UL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode: 11111100110111010000101001111110

rrc_MessageSequenceNumber: 1

message:

securityModeComplete:

rrc_TransactionIdentifier: 0

ul_IntegProtActivationInfo:

rrc_MessageSequenceNumberList:

RRC_MessageSequenceNumberList.element: 0

RRC_MessageSequenceNumberList.element: 0

RRC_MessageSequenceNumberList.element: 0

RRC_MessageSequenceNumberList.element: 0

RRC_MessageSequenceNumberList.element: 0

rb_UL_CiphActivationTimeInfo:

RB_ActivationTimeInfoList.element:

rb_Identity: 1

rlc_SequenceNumber: 0

RB_ActivationTimeInfoList.element:

rb_Identity: 2

rlc_SequenceNumber: 7

RB_ActivationTimeInfoList.element:

rb_Identity: 3

rlc_SequenceNumber: 6

RB_ActivationTimeInfoList.element:

rb_Identity: 4

rlc_SequenceNumber: 0

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]FE 6E 85 3F 0D 31 00 00
[8]01 80 00 02 00 E2 00 61
[16]80 00

#### CMAC Integrity Check Result

MAC RRC @ 00:01:45.450

Message Details:

Integrity Check Result:

MAC-I:11111100110111010000101001111110
Data:

[0]FC DD 0A 7E

#### RLC_AM_DATA_IND

LLA RRC @ 00:01:45.450

Channel ID: Rb2
Cell ID: -1

Message Details:

RLC_AM_DATA_IND:

cellId:-1

routingInfo:

rB_Identity:2

integrityResult:

integrityUsed (IntegrityStatus):i_pass

aM_message:

uL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode:11111100110111010000101001111110
rrc_MessageSequenceNumber:1

message: (UL_DCCH_MessageType)

securityModeComplete:

rrc_TransactionIdentifier:0

ul_IntegProtActivationInfo: (IntegrityProtActivationInfo)

rrc_MessageSequenceNumberList:

RRC_MessageSequenceNumber:0
RRC_MessageSequenceNumber:0
RRC_MessageSequenceNumber:0
RRC_MessageSequenceNumber:0
RRC_MessageSequenceNumber:0

rb_UL_CiphActivationTimeInfo: (RB_ActivationTimeInfoList)

RB_ActivationTimeInfo:

rb_Identity:1
rlc_SequenceNumber:0

RB_ActivationTimeInfo:

rb_Identity:2
rlc_SequenceNumber:7

RB_ActivationTimeInfo:

rb_Identity:3
rlc_SequenceNumber:6

RB_ActivationTimeInfo:

rb_Identity:4
rlc_SequenceNumber:0

laterNonCriticalExtensions: Omit

#### CRLC_Ciphering_Activate_REQ

RRC LLA @ 00:01:45.450

Cell ID: -1

Message Details:

CRLC_Ciphering_Activate_REQ:

cellId:-1
ratType:fdd
cn_DomainIdentity:ps_domain

ciphActivationInfo:

rb_UL_CipheringActivationTimeInfo: (RB_ActivationTimeInfoList)

RB_ActivationTimeInfo:

rb_Identity:1
rlc_SequenceNumber:0

RB_ActivationTimeInfo:

rb_Identity:2
rlc_SequenceNumber:7

RB_ActivationTimeInfo:

rb_Identity:3
rlc_SequenceNumber:6

RB_ActivationTimeInfo:

rb_Identity:4
rlc_SequenceNumber:0

incHFN (RLC_IncMode):notInc

#### CRLC UM Ciphering Activate REQ

LLA RLC @ 00:01:45.470

BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 60

Message Details:

Ciphering Parameters:

Mode command:Stop
Type:UM
Radio Bearer identity:0
Downlink activation time:0
Uplink activation time:0

#### CRLC UM Ciphering Activate CNF

RLC LLA @ 00:01:45.470

BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 60

Message Details:

#### CRLC AM Ciphering Activate REQ

LLA RLC @ 00:01:45.470

BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 60

Message Details:

Ciphering Parameters:

Mode command:Stop
Type:AM
Radio Bearer identity:1
Downlink activation time:2
Uplink activation time:7

#### CRLC AM Ciphering Activate CNF

RLC LLA @ 00:01:45.470

BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 60

Message Details:

#### CRLC AM Ciphering Activate REQ

LLA RLC @ 00:01:45.490

BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 62

Message Details:

Ciphering Parameters:

Mode command:Stop
Type:AM
Radio Bearer identity:2
Downlink activation time:3
Uplink activation time:6

#### CRLC AM Ciphering Activate CNF

RLC LLA @ 00:01:45.490

BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 62

Message Details:

#### CRLC_Ciphering_Activate_CNF

LLA RRC @ 00:01:45.510

Cell ID: -1

Message Details:

CRLC_Ciphering_Activate_CNF:

cellId:-1

#### CRLC_Integrity_Activate_REQ

RRC LLA @ 00:01:45.510

Cell ID: -1

Message Details:

CRLC_Integrity_Activate_REQ:

cellId:-1
cn_DomainIdentity:ps_domain

integrityActivationInfo:

ul_IntegProtActivationInfo: (IntegrityProtActivationInfoList)

SS_IntegrityProtActivationTimeInfo:

rb_Identity:0
rrc_MessageSequenceNumber:0

SS_IntegrityProtActivationTimeInfo:

rb_Identity:1
rrc_MessageSequenceNumber:0

SS_IntegrityProtActivationTimeInfo:

rb_Identity:3
rrc_MessageSequenceNumber:0

SS_IntegrityProtActivationTimeInfo:

rb_Identity:4
rrc_MessageSequenceNumber:0

#### CRLC AM Ciphering Activate REQ

LLA RLC @ 00:01:45.510

BTS unit: 1:1
Channel No: 4 Name: DCCH
CFN: 64

Message Details:

Ciphering Parameters:

Mode command:Stop
Type:AM
Radio Bearer identity:3
Downlink activation time:0
Uplink activation time:0

#### CRLC AM Ciphering Activate CNF

RLC LLA @ 00:01:45.510

BTS unit: 1:1
Channel No: 4 Name: DCCH
CFN: 64

Message Details:

#### CRLC_Integrity_Activate_CNF

LLA RRC @ 00:01:45.530

Cell ID: -1

Message Details:

CRLC_Integrity_Activate_CNF:

cellId:-1

#### CRLC_Resume_REQ

RRC LLA @ 00:01:45.530

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Resume_REQ:

cellId:-1

routingInfo:

rB_Identity:1

#### CRLC_Resume_CNF

LLA RRC @ 00:01:45.540

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Resume_CNF:

cellId:-1

routingInfo:

rB_Identity:1

#### CRLC_Resume_REQ

RRC LLA @ 00:01:45.540

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Resume_REQ:

cellId:-1

routingInfo:

rB_Identity:3

#### CRLC Resume REQ

LLA RLC @ 00:01:45.540

BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 67

Message Details:

#### CRLC Resume CNF

RLC LLA @ 00:01:45.540

BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 67

Message Details:

#### CRLC Resume REQ

LLA RLC @ 00:01:45.550

BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 68

Message Details:

#### CRLC Resume CNF

RLC LLA @ 00:01:45.550

BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 68

Message Details:

#### CRLC_Resume_CNF

LLA RRC @ 00:01:45.560

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Resume_CNF:

cellId:-1

routingInfo:

rB_Identity:3

#### CRLC_Resume_REQ

RRC LLA @ 00:01:45.560

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Resume_REQ:

cellId:-1

routingInfo:

rB_Identity:4

#### CRLC Resume REQ

LLA RLC @ 00:01:45.570

BTS unit: 1:1
Channel No: 4 Name: DCCH
CFN: 70

Message Details:

#### CRLC Resume CNF

RLC LLA @ 00:01:45.570

BTS unit: 1:1
Channel No: 4 Name: DCCH
CFN: 70

Message Details:

#### CMAC Integrity Check Request

RRC MAC @ 00:01:45.580

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000001
Data:

[0]00 00 00 01
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:1 (RNC to UE)
Message Length (bits):232
Message:

[0]80 00 00 01 81 42 02 81
[8]01 20 09 20 1E 22 00 00
[16]20 A3 35 62 46 83 00 BE
[24]82 46 8A CF 00

#### CMAC Integrity Check Result

MAC RRC @ 00:01:45.580

Message Details:

Integrity Check Result:

MAC-I:00110001101100010001110100011101
Data:

[0]31 B1 1D 1D

#### CRLC_Resume_CNF

LLA RRC @ 00:01:45.580

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Resume_CNF:

cellId:-1

routingInfo:

rB_Identity:4

#### RRC_DATA_REQ: gmm:routingAreaUpdateAccept

NAS RRC @ 00:01:45.580

Cell ID: -1

Message Details:

ROUTINGAREAUPDATEACCEPT:

skipIndicator: 0000

gMMProtocolDiscriminator: 1000

msgType: 00001001

updateResult:

spare: 0

value: 000

forceToStandby:

spare: 0

value: 000

periodicRAupdateTimer:

unit: 010

value: 01001

rai:

plmn: 00F110

lac: 0001

rac: 05

ptmsiSignature:

iei: 00011001

value: AB1234

allocatedPTMSI:

iei: 00011000

iel: 05

iDigit1: 1111

oddEvenInd: 0

typeOfId: 100

otherDigits: 12345678

msIdentity: Omitted

listNPDUnumbers: Omitted

readyTimer: Omitted

gmmCause: Omitted

t3302Value: Omitted

cellNotification: Omitted

equivalentPLMN: Omitted

pDP_ContextStatus: Omitted

#### RLC_AM_DATA_REQ:downlinkDirectTransfer

RRC RLC @ 00:01:45.580

Channel No: 3 Name: DCCH

Message Details:

Opt1: 0

Opt2: 0

DL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode: 00110001101100010001110100011101

rrc_MessageSequenceNumber: 1

message:

downlinkDirectTransfer:

r3:

downlinkDirectTransfer_r3:

rrc_TransactionIdentifier: 0

cn_DomainIdentity: ps_domain_CN_DomainIdentity [enum=1]

nas_Message: 0809004900F11000010519AB12341805F412345678

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]98 D8 8E 8E 89 42 02 81
[8]01 20 09 20 1E 22 00 00
[16]20 A3 35 62 46 83 00 BE
[24]82 46 8A CF 00

#### MAC_DATA_REQ

RLC MAC @ 00:01:45.590

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 72

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 18 98 D8 8E 8E 89 42
[8]02 81 01 20 09 20 1E 22
[16]00 00

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:3
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]98 D8 8E 8E 89 42 02 81
[8]01 20 09 20 1E 22 00 00

#### MAC_DATA_REQ

RLC MAC @ 00:01:45.590

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 72

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 25 1B FE 20 A3 35 62
[8]46 83 00 BE 82 46 8A CF
[16]00 00

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:4
Polling bit:1 (request a status report)
Length indicator 0 (octets):13
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (13 octets):

[0]20 A3 35 62 46 83 00 BE
[8]82 46 8A CF 00
Padding associated with length indicator 1 (1 octets):

[0]00

#### PHY_DATA_REQ

MAC PHY @ 00:01:45.600

BTS unit: 1:2
Channel No: 0 Name: FACH
CFN: 73

Message Details:

TFI:2
TB set size:336
TB size:168
TB set (raw, each TB word aligned):

[0]D0 00 12 80 18 98 D8 8E
[8]8E 89 42 02 81 01 20 09
[16]20 1E 22 00 00 00 D0 00
[24]12 80 25 1B FE 20 A3 35
[32]62 46 83 00 BE 82 46 8A
[40]CF 00 00 00

TB set (decoded):

TB 0:

TCTF:3
UEID type:C-RNTI
UEID:1
C/T:2
MAC SDU (144 bits):

[0]80 18 98 D8 8E 8E 89 42
[8]02 81 01 20 09 20 1E 22
[16]00 00

TB 1:

TCTF:3
UEID type:C-RNTI
UEID:1
C/T:2
MAC SDU (144 bits):

[0]80 25 1B FE 20 A3 35 62
[8]46 83 00 BE 82 46 8A CF
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:01:45.850

BTS unit: 1:2
Channel No: 0 Name: U_RACH
CFN: 78

Message Details:

TFI:0
TB set size:168
TB size:168
TB set (raw):

[0]50 00 12 02 00 50 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00 00 00

TB set (decoded):

TB 0:

TCTF:1
UEID type:C-RNTI
UEID:1
C/T:2
MAC SDU (144 bits):

[0]02 00 50 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### MAC_DATA_IND

MAC RLC @ 00:01:45.850

Category: Configuration
BTS unit: 1:2
Channel No: 3 Name: DCCH
CFN: 78

Message Details:

RLC PDU size (bits):142
RLC PDU (raw):

[0]02 00 50 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:5

#### PHY_DATA_IND

PHY MAC @ 00:01:45.900

BTS unit: 1:2
Channel No: 0 Name: U_RACH
CFN: 83

Message Details:

TFI:0
TB set size:168
TB size:168
TB set (raw):

[0]50 00 12 80 35 15 FE 84
[8]6B 8D 5C 0E C8 00 84 05
[16]00 55 55 55 55 00

TB set (decoded):

TB 0:

TCTF:1
UEID type:C-RNTI
UEID:1
C/T:2
MAC SDU (144 bits):

[0]80 35 15 FE 84 6B 8D 5C
[8]0E C8 00 84 05 00 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:01:45.900

Category: Configuration
BTS unit: 1:2
Channel No: 3 Name: DCCH
CFN: 83

Message Details:

RLC PDU size (bits):142
RLC PDU (raw):

[0]80 35 15 FE 84 6B 8D 5C
[8]0E C8 00 84 05 00 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:6
Polling bit:1 (request a status report)
Length indicator 0 (octets):10
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (10 octets):

[0]84 6B 8D 5C 0E C8 00 84
[8]05 00
Padding associated with length indicator 1 (4 octets):

[0]55 55 55 55

#### RLC_AM_DATA_IND: uplinkDirectTransfer

RLC RRC @ 00:01:45.910

Channel No: 3 Name: DCCH

Message Details:

UL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode: 00001000110101110001101010111000

rrc_MessageSequenceNumber: 1

message:

uplinkDirectTransfer:

cn_DomainIdentity: ps_domain_CN_DomainIdentity [enum=1]

nas_Message: 080A

measuredResultsOnRACH: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]84 6B 8D 5C 0E C8 00 84
[8]05 00

#### RRC_DATA_IND: gmm:routingAreaUpdateComplete

RRC NAS @ 00:01:45.910

Cell ID: -1

Message Details:

ROUTING_AREA_UPDATE_COMPLETE:

skipIndicator: 0000

gMMProtocolDiscriminator: 1000

msgType: 00001010

listNPDUnumbers: Omitted

#### MAC_DATA_REQ

RLC MAC @ 00:01:45.910

Category: Configuration
BTS unit: 1:2
Channel No: 3 Name: DCCH
CFN: 104

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 70 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:7

#### PHY_DATA_REQ

MAC PHY @ 00:01:45.910

BTS unit: 1:2
Channel No: 0 Name: FACH
CFN: 104

Message Details:

TFI:1
TB set size:168
TB size:168
TB set (raw):

[0]D0 00 12 02 00 70 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00 00 00

TB set (decoded):

TB 0:

TCTF:3
UEID type:C-RNTI
UEID:1
C/T:2
MAC SDU (144 bits):

[0]02 00 70 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### CMAC Integrity Check Request

RRC MAC @ 00:01:45.940

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000001
Data:

[0]00 00 00 01
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:0 (UE to RNC)
Message Length (bits):80
Message:

[0]80 00 00 01 86 C8 00 84
[8]05 00

#### CMAC Integrity Check Result

MAC RRC @ 00:01:45.940

Message Details:

Integrity Check Result:

MAC-I:00001000110101110001101010111000
Data:

[0]08 D7 1A B8

#### CMAC Integrity Check Request

RRC MAC @ 00:01:46.950

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000001
Data:

[0]00 00 00 01
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:1 (RNC to UE)
Message Length (bits):56
Message:

[0]80 00 00 00 83 C0 00

#### CMAC Integrity Check Result

MAC RRC @ 00:01:46.950

Message Details:

Integrity Check Result:

MAC-I:10000001111010010001000100010101
Data:

[0]81 E9 11 15

#### RLC_UM_DATA_REQ

RRC LLA @ 00:01:46.950

Channel ID: Rb1
Cell ID: -1

Message Details:

RLC_UM_DATA_REQ:

cellId:-1

routingInfo:

rB_Identity:1

uM_message:

dL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode:00000000000000000000000000000000
rrc_MessageSequenceNumber:0

message: (DL_DCCH_MessageType)

rrcConnectionRelease:

r3:

rrcConnectionRelease_r3: (RRCConnectionRelease_r3_IEs)

rrc_TransactionIdentifier:0
n_308: Omit
releaseCause:normalEvent

rplmn_information: Omit

laterNonCriticalExtensions: Omit

specialLI:false

#### RLC_UM_DATA_REQ: rrcConnectionRelease

LLA RLC @ 00:01:46.950

Channel No: 1 Name: DCCH

Message Details:

DL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode: 10000001111010010001000100010101

rrc_MessageSequenceNumber: 1

message:

rrcConnectionRelease:

r3:

rrcConnectionRelease_r3:

rrc_TransactionIdentifier: 0

n_308: Omitted

releaseCause: normalEvent_ReleaseCause [enum=0]

rplmn_information: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]C0 F4 88 8A 8B C0 00

#### MAC_DATA_REQ

RLC MAC @ 00:01:46.960

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 209

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]01 0F FE C0 F4 88 8A 8B
[8]C0 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

Sequence number:0
Length indicator 0 (octets):7
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (7 octets):

[0]C0 F4 88 8A 8B C0 00
Padding associated with length indicator 1 (8 octets):

[0]00 00 00 00 00 00 00 00

#### PHY_DATA_REQ

MAC PHY @ 00:01:46.970

BTS unit: 1:2
Channel No: 0 Name: FACH
CFN: 210

Message Details:

TFI:1
TB set size:168
TB size:168
TB set (raw):

[0]D0 00 10 01 0F FE C0 F4
[8]88 8A 8B C0 00 00 00 00
[16]00 00 00 00 00 00

TB set (decoded):

TB 0:

TCTF:3
UEID type:C-RNTI
UEID:1
C/T:0
MAC SDU (144 bits):

[0]01 0F FE C0 F4 88 8A 8B
[8]C0 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:01:47.280

BTS unit: 1:2
Channel No: 0 Name: U_RACH
CFN: 221

Message Details:

TFI:0
TB set size:168
TB size:168
TB set (raw):

[0]50 00 11 80 25 0D FE 8E
[8]50 3A A3 94 40 55 55 55
[16]55 55 55 55 55 00

TB set (decoded):

TB 0:

TCTF:1
UEID type:C-RNTI
UEID:1
C/T:1
MAC SDU (144 bits):

[0]80 25 0D FE 8E 50 3A A3
[8]94 40 55 55 55 55 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:01:47.280

Category: Configuration
BTS unit: 1:2
Channel No: 2 Name: DCCH
CFN: 221

Message Details:

RLC PDU size (bits):142
RLC PDU (raw):

[0]80 25 0D FE 8E 50 3A A3
[8]94 40 55 55 55 55 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:4
Polling bit:1 (request a status report)
Length indicator 0 (octets):6
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (6 octets):

[0]8E 50 3A A3 94 40
Padding associated with length indicator 1 (8 octets):

[0]55 55 55 55 55 55 55 55

#### MAC_DATA_REQ

RLC MAC @ 00:01:47.290

Category: Configuration
BTS unit: 1:2
Channel No: 2 Name: DCCH
CFN: 242

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 50 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:5

#### PHY_DATA_REQ

MAC PHY @ 00:01:47.290

BTS unit: 1:2
Channel No: 0 Name: FACH
CFN: 242

Message Details:

TFI:1
TB set size:168
TB size:168
TB set (raw):

[0]D0 00 11 02 00 50 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00 00 00

TB set (decoded):

TB 0:

TCTF:3
UEID type:C-RNTI
UEID:1
C/T:1
MAC SDU (144 bits):

[0]02 00 50 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### CMAC Integrity Check Request

RRC MAC @ 00:01:47.310

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000010
Data:

[0]00 00 00 02
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:0 (UE to RNC)
Message Length (bits):48
Message:

[0]80 00 00 01 04 40

#### RLC_AM_DATA_IND: rrcConnectionReleaseComplete

RLC LLA @ 00:01:47.310

Channel No: 2 Name: DCCH

Message Details:

UL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode: 00011100101000000111010101000111

rrc_MessageSequenceNumber: 2

message:

rrcConnectionReleaseComplete:

rrc_TransactionIdentifier: 0

errorIndication: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]8E 50 3A A3 94 40

#### CMAC Integrity Check Result

MAC RRC @ 00:01:47.310

Message Details:

Integrity Check Result:

MAC-I:00011100101000000111010101000111
Data:

[0]1C A0 75 47

#### RLC_AM_DATA_IND

LLA RRC @ 00:01:47.310

Channel ID: Rb2
Cell ID: -1

Message Details:

RLC_AM_DATA_IND:

cellId:-1

routingInfo:

rB_Identity:2

integrityResult:

integrityUsed (IntegrityStatus):i_pass

aM_message:

uL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode:00011100101000000111010101000111
rrc_MessageSequenceNumber:2

message: (UL_DCCH_MessageType)

rrcConnectionReleaseComplete:

rrc_TransactionIdentifier:0

errorIndication: (FailureCauseWithProtErr) Omit

laterNonCriticalExtensions: Omit

#### CRLC_Config_REQ

RRC LLA @ 00:01:48.330

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:1

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC UM Channel Release REQ

LLA RLC @ 00:01:48.330

BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 90

Message Details:

#### CRLC UM Channel Release CNF

RLC LLA @ 00:01:48.330

BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 90

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:01:48.340

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:1

#### CRLC_Config_REQ

RRC LLA @ 00:01:48.340

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:2

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC AM Channel Release REQ

LLA RLC @ 00:01:48.350

BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 92

Message Details:

#### CRLC AM Channel Release CNF

RLC LLA @ 00:01:48.350

BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 92

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:01:48.360

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:2

#### CRLC_Config_REQ

RRC LLA @ 00:01:48.360

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:3

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC_Config_CNF

LLA RRC @ 00:01:48.370

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:3

#### CRLC_Config_REQ

RRC LLA @ 00:01:48.370

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:4

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC AM Channel Release REQ

LLA RLC @ 00:01:48.370

BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 94

Message Details:

#### CRLC AM Channel Release CNF

RLC LLA @ 00:01:48.370

BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 94

Message Details:

#### CRLC AM Channel Release REQ

LLA RLC @ 00:01:48.380

BTS unit: 1:1
Channel No: 4 Name: DCCH
CFN: 95

Message Details:

#### CRLC AM Channel Release CNF

RLC LLA @ 00:01:48.380

BTS unit: 1:1
Channel No: 4 Name: DCCH
CFN: 95

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:01:48.390

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:4

#### CRLC_Config_REQ

RRC LLA @ 00:01:48.390

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:1

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode)

dl_UM_RLC_Mode:

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):136

dl_RLCModeInfo: (UL_RLC_Mode)

ul_UM_RLC_Mode:

transmissionRLC_Discard:

timerBasedNoExplicit (NoExplicitDiscard):dt100

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity):1
dLlogicalChannelIdentity (LogicalChannelIdentity):1
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC_Config_CNF

LLA RRC @ 00:01:48.400

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:1

#### CRLC_Config_REQ

RRC LLA @ 00:01:48.400

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:2

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode)

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):128

dl_RLCModeInfo: (UL_RLC_Mode)

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp400
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity):2
dLlogicalChannelIdentity (LogicalChannelIdentity):2
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC UM Channel Establish REQ

LLA RLC @ 00:01:48.400

BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 97

Message Details:

Configuration Parameters:

PU Size In Bits:136

#### CRLC UM Channel Establish CNF

RLC LLA @ 00:01:48.400

BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 97

Message Details:

#### CRLC AM Channel Establish REQ

LLA RLC @ 00:01:48.410

BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 98

Message Details:

Configuration Parameters:

PU Size In Bits:128

Timer Parameters:

Poll (ms):400
Poll Prohibit (ms):0
EPC (ms):0
Discard (ms):0
Poll Periodic (ms):0
Status Prohibit (ms):0
Status Periodic (ms):0
Reset (ms):500
MRW (ms):0

Protocol Parameters:

Max Dat:15
Poll PU:0
Poll SDU:1
Poll Window:99
Max Reset:1
Tx Window Size:32
Rx Window Size:32
Max MRW:0
SDU Discard Mode:No discard

Polling Triggers:

Last PU In Buffer:On
Last PU In Retransmission Buffer:On
Poll Timer:On
Every Poll-PU PU:Off
Every Poll-SDU SDU:On
Poll-Window Percent Of Transmission Buffer:On
Timer Based:Off

Status Triggers:

Missing PU:On
Timer Based:Off
EPC Mechanism:Off

#### CRLC AM Channel Establish CNF

RLC LLA @ 00:01:48.410

BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 98

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:01:48.420

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:2

#### CRLC_Config_REQ

RRC LLA @ 00:01:48.420

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:3

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode)

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):128

dl_RLCModeInfo: (UL_RLC_Mode)

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp400
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity):3
dLlogicalChannelIdentity (LogicalChannelIdentity):3
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC AM Channel Establish REQ

LLA RLC @ 00:01:48.430

BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 100

Message Details:

Configuration Parameters:

PU Size In Bits:128

Timer Parameters:

Poll (ms):400
Poll Prohibit (ms):0
EPC (ms):0
Discard (ms):0
Poll Periodic (ms):0
Status Prohibit (ms):0
Status Periodic (ms):0
Reset (ms):500
MRW (ms):0

Protocol Parameters:

Max Dat:15
Poll PU:0
Poll SDU:1
Poll Window:99
Max Reset:1
Tx Window Size:32
Rx Window Size:32
Max MRW:0
SDU Discard Mode:No discard

Polling Triggers:

Last PU In Buffer:On
Last PU In Retransmission Buffer:On
Poll Timer:On
Every Poll-PU PU:Off
Every Poll-SDU SDU:On
Poll-Window Percent Of Transmission Buffer:On
Timer Based:Off

Status Triggers:

Missing PU:On
Timer Based:Off
EPC Mechanism:Off

#### CRLC AM Channel Establish CNF

RLC LLA @ 00:01:48.430

BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 100

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:01:48.440

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:3

#### CRLC_Config_REQ

RRC LLA @ 00:01:48.440

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:4

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode)

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):128

dl_RLCModeInfo: (UL_RLC_Mode)

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp400
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity):4
dLlogicalChannelIdentity (LogicalChannelIdentity):4
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC AM Channel Establish REQ

LLA RLC @ 00:01:48.440

BTS unit: 1:1
Channel No: 4 Name: DCCH
CFN: 101

Message Details:

Configuration Parameters:

PU Size In Bits:128

Timer Parameters:

Poll (ms):400
Poll Prohibit (ms):0
EPC (ms):0
Discard (ms):0
Poll Periodic (ms):0
Status Prohibit (ms):0
Status Periodic (ms):0
Reset (ms):500
MRW (ms):0

Protocol Parameters:

Max Dat:15
Poll PU:0
Poll SDU:1
Poll Window:99
Max Reset:1
Tx Window Size:32
Rx Window Size:32
Max MRW:0
SDU Discard Mode:No discard

Polling Triggers:

Last PU In Buffer:On
Last PU In Retransmission Buffer:On
Poll Timer:On
Every Poll-PU PU:Off
Every Poll-SDU SDU:On
Poll-Window Percent Of Transmission Buffer:On
Timer Based:Off

Status Triggers:

Missing PU:On
Timer Based:Off
EPC Mechanism:Off

#### CRLC AM Channel Establish CNF

RLC LLA @ 00:01:48.440

BTS unit: 1:1
Channel No: 4 Name: DCCH
CFN: 101

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:01:48.450

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:4

#### CRLC_Config_REQ

RRC LLA @ 00:01:48.450

Channel ID: Rb0
Cell ID: 0

Message Details:

CRLC_Config_REQ:

cellId:0

routingInfo:

rB_Identity:0

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC UM Channel Release REQ

LLA RLC @ 00:01:48.460

BTS unit: 1:1
Channel No: 1 Name: CCCH
CFN: 103

Message Details:

#### CRLC UM Channel Release CNF

RLC LLA @ 00:01:48.460

BTS unit: 1:1
Channel No: 1 Name: CCCH
CFN: 103

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:01:48.470

Channel ID: Rb0
Cell ID: 0

Message Details:

CRLC_Config_CNF:

cellId:0

routingInfo:

rB_Identity:0

#### CMAC_Config_REQ

RRC LLA @ 00:01:48.470

Channel ID: PRACH#1
Cell ID: 0

Message Details:

CMAC_Config_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:8

ratType:fdd

configMessage:

release:

#### CMAC Configuration REQ

LLA MAC @ 00:01:48.480

BTS unit: 1:1
Channel No: 0 Name: PRACH
CFN: 105

Message Details:

Configuration Parameters:

Number Of Transport Channels:0
Active Flag:0

Transport Format Combination Set:

Number Of Transport Format Combinations:0

#### CMAC Configuration CNF

MAC LLA @ 00:01:48.480

BTS unit: 1:1
Channel No: 0 Name: PRACH
CFN: 105

Message Details:

#### CMAC_Config_CNF

LLA RRC @ 00:01:48.500

Channel ID: PRACH#1
Cell ID: 0

Message Details:

CMAC_Config_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:8

#### CPHY_TrCH_Release_REQ

RRC LLA @ 00:01:48.500

Channel ID: PRACH#1
Cell ID: 0

Message Details:

CPHY_TrCH_Release_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:8

trchConfigType:

nonDch:

#### CPHY_TrCH_Release_CNF

LLA RRC @ 00:01:48.510

Channel ID: PRACH#1
Cell ID: 0

Message Details:

CPHY_TrCH_Release_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:8

#### CPHY_RL_Release_REQ

RRC LLA @ 00:01:48.510

Channel ID: AICH#1
Cell ID: 0

Message Details:

CPHY_RL_Release_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:7

#### CPHY Transport Channel Release REQ

LLA PHY @ 00:01:48.510

BTS unit: 1:1
Channel No: 0 Name: PRACH
CFN: 108

Message Details:

#### CPHY Transport Channel Release CNF

PHY LLA @ 00:01:48.510

BTS unit: 1:1
Channel No: 0 Name: PRACH
CFN: 108

Message Details:

#### CPHY Radio Link Release REQ

LLA PHY @ 00:01:48.520

BTS unit: 1:1
Channel No: 0 Name: AICH
CFN: 109

Message Details:

#### CPHY Radio Link Release CNF

PHY LLA @ 00:01:48.520

BTS unit: 1:1
Channel No: 0 Name: AICH
CFN: 109

Message Details:

#### CPHY_RL_Release_CNF

LLA RRC @ 00:01:48.530

Channel ID: AICH#1
Cell ID: 0

Message Details:

CPHY_RL_Release_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:7

#### CPHY_RL_Release_REQ

RRC LLA @ 00:01:48.530

Channel ID: PRACH#1
Cell ID: 0

Message Details:

CPHY_RL_Release_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:8

#### CPHY_RL_Release_CNF

LLA RRC @ 00:01:48.540

Channel ID: PRACH#1
Cell ID: 0

Message Details:

CPHY_RL_Release_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:8

#### CRLC_Config_REQ

RRC LLA @ 00:01:48.540

Channel ID: RbPcch
Cell ID: 0

Message Details:

CRLC_Config_REQ:

cellId:0

routingInfo:

rB_Identity:-2

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CPHY Radio Link Release REQ

LLA PHY @ 00:01:48.540

BTS unit: 1:1
Channel No: 0 Name: PRACH
CFN: 111

Message Details:

#### CPHY Radio Link Release CNF

PHY LLA @ 00:01:48.540

BTS unit: 1:1
Channel No: 0 Name: PRACH
CFN: 111

Message Details:

#### CRLC TM Channel Release REQ

LLA RLC @ 00:01:48.550

BTS unit: 1:1
Channel No: 0 Name: PCCH
CFN: 112

Message Details:

#### CRLC TM Channel Release CNF

RLC LLA @ 00:01:48.550

BTS unit: 1:1
Channel No: 0 Name: PCCH
CFN: 112

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:01:48.560

Channel ID: RbPcch
Cell ID: 0

Message Details:

CRLC_Config_CNF:

cellId:0

routingInfo:

rB_Identity:-2

#### CMAC_Config_REQ

RRC LLA @ 00:01:48.560

Channel ID: S-CCPCH#1
Cell ID: 0

Message Details:

CMAC_Config_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:5

ratType:fdd

configMessage:

release:

#### CMAC_Config_CNF

LLA RRC @ 00:01:48.580

Channel ID: S-CCPCH#1
Cell ID: 0

Message Details:

CMAC_Config_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:5

#### CPHY_TrCH_Release_REQ

RRC LLA @ 00:01:48.580

Channel ID: S-CCPCH#1
Cell ID: 0

Message Details:

CPHY_TrCH_Release_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:5

trchConfigType:

nonDch:

#### CPHY Transport Channel Release REQ

LLA PHY @ 00:01:48.580

BTS unit: 1:1
Channel No: 0 Name: S_CCPCH
CFN: 115

Message Details:

#### CPHY Transport Channel Release CNF

PHY LLA @ 00:01:48.580

BTS unit: 1:1
Channel No: 0 Name: S_CCPCH
CFN: 115

Message Details:

#### CPHY_TrCH_Release_CNF

LLA RRC @ 00:01:48.590

Channel ID: S-CCPCH#1
Cell ID: 0

Message Details:

CPHY_TrCH_Release_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:5

#### CPHY_RL_Release_REQ

RRC LLA @ 00:01:48.590

Channel ID: PICH#1
Cell ID: 0

Message Details:

CPHY_RL_Release_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:6

#### CPHY Radio Link Release REQ

LLA PHY @ 00:01:48.600

BTS unit: 1:1
Channel No: 0 Name: PICH
CFN: 117

Message Details:

#### CPHY Radio Link Release CNF

PHY LLA @ 00:01:48.600

BTS unit: 1:1
Channel No: 0 Name: PICH
CFN: 117

Message Details:

#### CPHY_RL_Release_CNF

LLA RRC @ 00:01:48.610

Channel ID: PICH#1
Cell ID: 0

Message Details:

CPHY_RL_Release_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:6

#### CPHY_RL_Release_REQ

RRC LLA @ 00:01:48.610

Channel ID: S-CCPCH#1
Cell ID: 0

Message Details:

CPHY_RL_Release_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:5

#### CPHY_RL_Release_CNF

LLA RRC @ 00:01:48.620

Channel ID: S-CCPCH#1
Cell ID: 0

Message Details:

CPHY_RL_Release_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:5

#### CRLC_Config_REQ

RRC LLA @ 00:01:48.620

Channel ID: RbBcch
Cell ID: 0

Message Details:

CRLC_Config_REQ:

cellId:0

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CPHY Radio Link Release REQ

LLA PHY @ 00:01:48.620

BTS unit: 1:1
Channel No: 0 Name: S_CCPCH
CFN: 119

Message Details:

#### CPHY Radio Link Release CNF

PHY LLA @ 00:01:48.620

BTS unit: 1:1
Channel No: 0 Name: S_CCPCH
CFN: 119

Message Details:

#### CRLC TM Channel Release REQ

LLA RLC @ 00:01:48.630

BTS unit: 1:1
Channel No: 0 Name: BCCH
CFN: 120

Message Details:

#### CRLC TM Channel Release CNF

RLC LLA @ 00:01:48.630

BTS unit: 1:1
Channel No: 0 Name: BCCH
CFN: 120

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:01:48.640

Channel ID: RbBcch
Cell ID: 0

Message Details:

CRLC_Config_CNF:

cellId:0

routingInfo:

rB_Identity:-1

#### CMAC_Config_REQ

RRC LLA @ 00:01:48.640

Channel ID: P-CCPCH
Cell ID: 0

Message Details:

CMAC_Config_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:4

ratType:fdd

configMessage:

release:

#### CMAC_Config_CNF

LLA RRC @ 00:01:48.650

Channel ID: P-CCPCH
Cell ID: 0

Message Details:

CMAC_Config_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:4

#### CPHY_TrCH_Release_REQ

RRC LLA @ 00:01:48.650

Channel ID: P-CCPCH
Cell ID: 0

Message Details:

CPHY_TrCH_Release_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:4

trchConfigType:

nonDch:

#### CMAC Configuration REQ

LLA MAC @ 00:01:48.650

BTS unit: 1:1
Channel No: 0 Name: P_CCPCH
CFN: 122

Message Details:

Configuration Parameters:

Number Of Transport Channels:0
Active Flag:0

Transport Format Combination Set:

Number Of Transport Format Combinations:0

#### CMAC Configuration CNF

MAC LLA @ 00:01:48.650

BTS unit: 1:1
Channel No: 0 Name: P_CCPCH
CFN: 122

Message Details:

#### CPHY Transport Channel Release REQ

LLA PHY @ 00:01:48.660

BTS unit: 1:1
Channel No: 0 Name: P_CCPCH
CFN: 123

Message Details:

#### CPHY Transport Channel Release CNF

PHY LLA @ 00:01:48.660

BTS unit: 1:1
Channel No: 0 Name: P_CCPCH
CFN: 123

Message Details:

#### CPHY_TrCH_Release_CNF

LLA RRC @ 00:01:48.670

Channel ID: P-CCPCH
Cell ID: 0

Message Details:

CPHY_TrCH_Release_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:4

#### CPHY_RL_Release_REQ

RRC LLA @ 00:01:48.670

Channel ID: S-SCH
Cell ID: 0

Message Details:

CPHY_RL_Release_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:2

#### CPHY Radio Link Release REQ

LLA PHY @ 00:01:48.680

BTS unit: 1:1
Channel No: 0 Name: S_SCH
CFN: 125

Message Details:

#### CPHY Radio Link Release CNF

PHY LLA @ 00:01:48.680

BTS unit: 1:1
Channel No: 0 Name: S_SCH
CFN: 125

Message Details:

#### CPHY_RL_Release_CNF

LLA RRC @ 00:01:48.690

Channel ID: S-SCH
Cell ID: 0

Message Details:

CPHY_RL_Release_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:2

#### CPHY_RL_Release_REQ

RRC LLA @ 00:01:48.690

Channel ID: P-SCH
Cell ID: 0

Message Details:

CPHY_RL_Release_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:1

#### CPHY Radio Link Release REQ

LLA PHY @ 00:01:48.690

BTS unit: 1:1
Channel No: 0 Name: P_SCH
CFN: 126

Message Details:

#### CPHY Radio Link Release CNF

PHY LLA @ 00:01:48.690

BTS unit: 1:1
Channel No: 0 Name: P_SCH
CFN: 126

Message Details:

#### CPHY_RL_Release_CNF

LLA RRC @ 00:01:48.700

Channel ID: P-SCH
Cell ID: 0

Message Details:

CPHY_RL_Release_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:1

#### CPHY_RL_Release_REQ

RRC LLA @ 00:01:48.700

Channel ID: P-CCPCH
Cell ID: 0

Message Details:

CPHY_RL_Release_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:4

#### CPHY Radio Link Release REQ

LLA PHY @ 00:01:48.710

BTS unit: 1:1
Channel No: 0 Name: P_CCPCH
CFN: 128

Message Details:

#### CPHY Radio Link Release CNF

PHY LLA @ 00:01:48.710

BTS unit: 1:1
Channel No: 0 Name: P_CCPCH
CFN: 128

Message Details:

#### CPHY_RL_Release_CNF

LLA RRC @ 00:01:48.720

Channel ID: P-CCPCH
Cell ID: 0

Message Details:

CPHY_RL_Release_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:4

#### CPHY_RL_Release_REQ

RRC LLA @ 00:01:48.720

Channel ID: P-CPICH
Cell ID: 0

Message Details:

CPHY_RL_Release_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:0

#### CPHY Radio Link Release REQ

LLA PHY @ 00:01:48.730

BTS unit: 1:1
Channel No: 0 Name: P_CPICH
CFN: 130

Message Details:

#### CPHY Radio Link Release CNF

PHY LLA @ 00:01:48.730

BTS unit: 1:1
Channel No: 0 Name: P_CPICH
CFN: 130

Message Details:

#### CRLC UM Channel Release REQ

LLA RLC @ 00:01:48.720

BTS unit: 2:1
Channel No: 1 Name: CCCH
CFN: 129

Message Details:

#### CRLC UM Channel Release CNF

RLC LLA @ 00:01:48.720

BTS unit: 2:1
Channel No: 1 Name: CCCH
CFN: 129

Message Details:

#### CMAC Configuration REQ

LLA MAC @ 00:01:48.740

BTS unit: 2:1
Channel No: 0 Name: PRACH
CFN: 131

Message Details:

Configuration Parameters:

Number Of Transport Channels:0
Active Flag:0

Transport Format Combination Set:

Number Of Transport Format Combinations:0

#### CMAC Configuration CNF

MAC LLA @ 00:01:48.740

BTS unit: 2:1
Channel No: 0 Name: PRACH
CFN: 131

Message Details:

#### CPHY_RL_Release_CNF

LLA RRC @ 00:01:48.750

Channel ID: P-CPICH
Cell ID: 0

Message Details:

CPHY_RL_Release_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:0

#### CRLC_Config_REQ

RRC LLA @ 00:01:48.750

Channel ID: Rb0
Cell ID: 3

Message Details:

CRLC_Config_REQ:

cellId:3

routingInfo:

rB_Identity:0

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC_Config_CNF

LLA RRC @ 00:01:48.760

Channel ID: Rb0
Cell ID: 3

Message Details:

CRLC_Config_CNF:

cellId:3

routingInfo:

rB_Identity:0

#### CMAC_Config_REQ

RRC LLA @ 00:01:48.760

Channel ID: PRACH#1
Cell ID: 3

Message Details:

CMAC_Config_REQ:

cellId:3

routingInfo:

physicalChannelIdentity:8

ratType:fdd

configMessage:

release:

#### CPHY Transport Channel Release REQ

LLA PHY @ 00:01:48.760

BTS unit: 2:1
Channel No: 0 Name: PRACH
CFN: 133

Message Details:

#### CPHY Transport Channel Release CNF

PHY LLA @ 00:01:48.760

BTS unit: 2:1
Channel No: 0 Name: PRACH
CFN: 133

Message Details:

#### CPHY Radio Link Release REQ

LLA PHY @ 00:01:48.780

BTS unit: 2:1
Channel No: 0 Name: AICH
CFN: 135

Message Details:

#### CPHY Radio Link Release CNF

PHY LLA @ 00:01:48.780

BTS unit: 2:1
Channel No: 0 Name: AICH
CFN: 135

Message Details:

#### CMAC_Config_CNF

LLA RRC @ 00:01:48.790

Channel ID: PRACH#1
Cell ID: 3

Message Details:

CMAC_Config_CNF:

cellId:3

routingInfo:

physicalChannelIdentity:8

#### CPHY_TrCH_Release_REQ

RRC LLA @ 00:01:48.790

Channel ID: PRACH#1
Cell ID: 3

Message Details:

CPHY_TrCH_Release_REQ:

cellId:3

routingInfo:

physicalChannelIdentity:8

trchConfigType:

nonDch:

#### CPHY Radio Link Release REQ

LLA PHY @ 00:01:48.800

BTS unit: 2:1
Channel No: 0 Name: PRACH
CFN: 137

Message Details:

#### CPHY Radio Link Release CNF

PHY LLA @ 00:01:48.800

BTS unit: 2:1
Channel No: 0 Name: PRACH
CFN: 137

Message Details:

#### CPHY_TrCH_Release_CNF

LLA RRC @ 00:01:48.810

Channel ID: PRACH#1
Cell ID: 3

Message Details:

CPHY_TrCH_Release_CNF:

cellId:3

routingInfo:

physicalChannelIdentity:8

#### CPHY_RL_Release_REQ

RRC LLA @ 00:01:48.810

Channel ID: AICH#1
Cell ID: 3

Message Details:

CPHY_RL_Release_REQ:

cellId:3

routingInfo:

physicalChannelIdentity:7

#### CPHY_RL_Release_CNF

LLA RRC @ 00:01:48.830

Channel ID: AICH#1
Cell ID: 3

Message Details:

CPHY_RL_Release_CNF:

cellId:3

routingInfo:

physicalChannelIdentity:7

#### CPHY_RL_Release_REQ

RRC LLA @ 00:01:48.830

Channel ID: PRACH#1
Cell ID: 3

Message Details:

CPHY_RL_Release_REQ:

cellId:3

routingInfo:

physicalChannelIdentity:8

#### CRLC TM Channel Release REQ

LLA RLC @ 00:01:48.830

BTS unit: 2:1
Channel No: 0 Name: PCCH
CFN: 140

Message Details:

#### CRLC TM Channel Release CNF

RLC LLA @ 00:01:48.830

BTS unit: 2:1
Channel No: 0 Name: PCCH
CFN: 140

Message Details:

#### CPHY_RL_Release_CNF

LLA RRC @ 00:01:48.860

Channel ID: PRACH#1
Cell ID: 3

Message Details:

CPHY_RL_Release_CNF:

cellId:3

routingInfo:

physicalChannelIdentity:8

#### CRLC_Config_REQ

RRC LLA @ 00:01:48.860

Channel ID: RbPcch
Cell ID: 3

Message Details:

CRLC_Config_REQ:

cellId:3

routingInfo:

rB_Identity:-2

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CPHY Transport Channel Release REQ

LLA PHY @ 00:01:48.860

BTS unit: 2:1
Channel No: 0 Name: S_CCPCH
CFN: 143

Message Details:

#### CPHY Transport Channel Release CNF

PHY LLA @ 00:01:48.860

BTS unit: 2:1
Channel No: 0 Name: S_CCPCH
CFN: 143

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:01:48.870

Channel ID: RbPcch
Cell ID: 3

Message Details:

CRLC_Config_CNF:

cellId:3

routingInfo:

rB_Identity:-2

#### CMAC_Config_REQ

RRC LLA @ 00:01:48.870

Channel ID: S-CCPCH#1
Cell ID: 3

Message Details:

CMAC_Config_REQ:

cellId:3

routingInfo:

physicalChannelIdentity:5

ratType:fdd

configMessage:

release:

#### CPHY Radio Link Release REQ

LLA PHY @ 00:01:48.870

BTS unit: 2:1
Channel No: 0 Name: PICH
CFN: 144

Message Details:

#### CPHY Radio Link Release CNF

PHY LLA @ 00:01:48.870

BTS unit: 2:1
Channel No: 0 Name: PICH
CFN: 144

Message Details:

#### CMAC_Config_CNF

LLA RRC @ 00:01:48.890

Channel ID: S-CCPCH#1
Cell ID: 3

Message Details:

CMAC_Config_CNF:

cellId:3

routingInfo:

physicalChannelIdentity:5

#### CPHY_TrCH_Release_REQ

RRC LLA @ 00:01:48.890

Channel ID: S-CCPCH#1
Cell ID: 3

Message Details:

CPHY_TrCH_Release_REQ:

cellId:3

routingInfo:

physicalChannelIdentity:5

trchConfigType:

nonDch:

#### CPHY Radio Link Release REQ

LLA PHY @ 00:01:48.890

BTS unit: 2:1
Channel No: 0 Name: S_CCPCH
CFN: 146

Message Details:

#### CPHY Radio Link Release CNF

PHY LLA @ 00:01:48.890

BTS unit: 2:1
Channel No: 0 Name: S_CCPCH
CFN: 146

Message Details:

#### CPHY_TrCH_Release_CNF

LLA RRC @ 00:01:48.900

Channel ID: S-CCPCH#1
Cell ID: 3

Message Details:

CPHY_TrCH_Release_CNF:

cellId:3

routingInfo:

physicalChannelIdentity:5

#### CPHY_RL_Release_REQ

RRC LLA @ 00:01:48.900

Channel ID: PICH#1
Cell ID: 3

Message Details:

CPHY_RL_Release_REQ:

cellId:3

routingInfo:

physicalChannelIdentity:6

#### CRLC TM Channel Release REQ

LLA RLC @ 00:01:48.900

BTS unit: 2:1
Channel No: 0 Name: BCCH
CFN: 147

Message Details:

#### CRLC TM Channel Release CNF

RLC LLA @ 00:01:48.900

BTS unit: 2:1
Channel No: 0 Name: BCCH
CFN: 147

Message Details:

#### CPHY_RL_Release_CNF

LLA RRC @ 00:01:48.920

Channel ID: PICH#1
Cell ID: 3

Message Details:

CPHY_RL_Release_CNF:

cellId:3

routingInfo:

physicalChannelIdentity:6

#### CPHY_RL_Release_REQ

RRC LLA @ 00:01:48.920

Channel ID: S-CCPCH#1
Cell ID: 3

Message Details:

CPHY_RL_Release_REQ:

cellId:3

routingInfo:

physicalChannelIdentity:5

#### CMAC Configuration REQ

LLA MAC @ 00:01:48.920

BTS unit: 2:1
Channel No: 0 Name: P_CCPCH
CFN: 149

Message Details:

Configuration Parameters:

Number Of Transport Channels:0
Active Flag:0

Transport Format Combination Set:

Number Of Transport Format Combinations:0

#### CMAC Configuration CNF

MAC LLA @ 00:01:48.920

BTS unit: 2:1
Channel No: 0 Name: P_CCPCH
CFN: 149

Message Details:

#### CPHY_RL_Release_CNF

LLA RRC @ 00:01:48.940

Channel ID: S-CCPCH#1
Cell ID: 3

Message Details:

CPHY_RL_Release_CNF:

cellId:3

routingInfo:

physicalChannelIdentity:5

#### CRLC_Config_REQ

RRC LLA @ 00:01:48.940

Channel ID: RbBcch
Cell ID: 3

Message Details:

CRLC_Config_REQ:

cellId:3

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CPHY Transport Channel Release REQ

LLA PHY @ 00:01:48.940

BTS unit: 2:1
Channel No: 0 Name: P_CCPCH
CFN: 151

Message Details:

#### CPHY Transport Channel Release CNF

PHY LLA @ 00:01:48.940

BTS unit: 2:1
Channel No: 0 Name: P_CCPCH
CFN: 151

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:01:48.950

Channel ID: RbBcch
Cell ID: 3

Message Details:

CRLC_Config_CNF:

cellId:3

routingInfo:

rB_Identity:-1

#### CMAC_Config_REQ

RRC LLA @ 00:01:48.950

Channel ID: P-CCPCH
Cell ID: 3

Message Details:

CMAC_Config_REQ:

cellId:3

routingInfo:

physicalChannelIdentity:4

ratType:fdd

configMessage:

release:

#### CMAC_Config_CNF

LLA RRC @ 00:01:48.970

Channel ID: P-CCPCH
Cell ID: 3

Message Details:

CMAC_Config_CNF:

cellId:3

routingInfo:

physicalChannelIdentity:4

#### CPHY_TrCH_Release_REQ

RRC LLA @ 00:01:48.970

Channel ID: P-CCPCH
Cell ID: 3

Message Details:

CPHY_TrCH_Release_REQ:

cellId:3

routingInfo:

physicalChannelIdentity:4

trchConfigType:

nonDch:

#### CPHY Radio Link Release REQ

LLA PHY @ 00:01:48.970

BTS unit: 2:1
Channel No: 0 Name: S_SCH
CFN: 154

Message Details:

#### CPHY Radio Link Release CNF

PHY LLA @ 00:01:48.970

BTS unit: 2:1
Channel No: 0 Name: S_SCH
CFN: 154

Message Details:

#### CPHY Radio Link Release REQ

LLA PHY @ 00:01:48.980

BTS unit: 2:1
Channel No: 0 Name: P_SCH
CFN: 155

Message Details:

#### CPHY Radio Link Release CNF

PHY LLA @ 00:01:48.980

BTS unit: 2:1
Channel No: 0 Name: P_SCH
CFN: 155

Message Details:

#### CPHY_TrCH_Release_CNF

LLA RRC @ 00:01:49.000

Channel ID: P-CCPCH
Cell ID: 3

Message Details:

CPHY_TrCH_Release_CNF:

cellId:3

routingInfo:

physicalChannelIdentity:4

#### CPHY_RL_Release_REQ

RRC LLA @ 00:01:49.000

Channel ID: S-SCH
Cell ID: 3

Message Details:

CPHY_RL_Release_REQ:

cellId:3

routingInfo:

physicalChannelIdentity:2

#### CPHY Radio Link Release REQ

LLA PHY @ 00:01:49.000

BTS unit: 2:1
Channel No: 0 Name: P_CCPCH
CFN: 157

Message Details:

#### CPHY Radio Link Release CNF

PHY LLA @ 00:01:49.000

BTS unit: 2:1
Channel No: 0 Name: P_CCPCH
CFN: 157

Message Details:

#### CPHY_RL_Release_CNF

LLA RRC @ 00:01:49.010

Channel ID: S-SCH
Cell ID: 3

Message Details:

CPHY_RL_Release_CNF:

cellId:3

routingInfo:

physicalChannelIdentity:2

#### CPHY_RL_Release_REQ

RRC LLA @ 00:01:49.010

Channel ID: P-SCH
Cell ID: 3

Message Details:

CPHY_RL_Release_REQ:

cellId:3

routingInfo:

physicalChannelIdentity:1

#### CPHY Radio Link Release REQ

LLA PHY @ 00:01:49.010

BTS unit: 2:1
Channel No: 0 Name: P_CPICH
CFN: 158

Message Details:

#### CPHY Radio Link Release CNF

PHY LLA @ 00:01:49.010

BTS unit: 2:1
Channel No: 0 Name: P_CPICH
CFN: 158

Message Details:

#### CPHY_RL_Release_CNF

LLA RRC @ 00:01:49.030

Channel ID: P-SCH
Cell ID: 3

Message Details:

CPHY_RL_Release_CNF:

cellId:3

routingInfo:

physicalChannelIdentity:1

#### CPHY_RL_Release_REQ

RRC LLA @ 00:01:49.030

Channel ID: P-CCPCH
Cell ID: 3

Message Details:

CPHY_RL_Release_REQ:

cellId:3

routingInfo:

physicalChannelIdentity:4

#### CPHY_RL_Release_CNF

LLA RRC @ 00:01:49.040

Channel ID: P-CCPCH
Cell ID: 3

Message Details:

CPHY_RL_Release_CNF:

cellId:3

routingInfo:

physicalChannelIdentity:4

#### CPHY_RL_Release_REQ

RRC LLA @ 00:01:49.040

Channel ID: P-CPICH
Cell ID: 3

Message Details:

CPHY_RL_Release_REQ:

cellId:3

routingInfo:

physicalChannelIdentity:0

#### CPHY_RL_Release_CNF

LLA RRC @ 00:01:49.060

Channel ID: P-CPICH
Cell ID: 3

Message Details:

CPHY_RL_Release_CNF:

cellId:3

routingInfo:

physicalChannelIdentity:0

#### CRLC_Config_REQ

RRC LLA @ 00:01:49.060

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:1

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC UM Channel Release REQ

LLA RLC @ 00:01:49.070

BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 164

Message Details:

#### CRLC UM Channel Release CNF

RLC LLA @ 00:01:49.070

BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 164

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:01:49.080

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:1

#### CRLC_Config_REQ

RRC LLA @ 00:01:49.080

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:2

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC AM Channel Release REQ

LLA RLC @ 00:01:49.080

BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 165

Message Details:

#### CRLC AM Channel Release CNF

RLC LLA @ 00:01:49.090

BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 166

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:01:49.090

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:2

#### CRLC_Config_REQ

RRC LLA @ 00:01:49.090

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:3

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC AM Channel Release REQ

LLA RLC @ 00:01:49.100

BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 167

Message Details:

#### CRLC AM Channel Release CNF

RLC LLA @ 00:01:49.100

BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 167

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:01:49.110

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:3

#### CRLC_Config_REQ

RRC LLA @ 00:01:49.110

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:4

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC_Config_CNF

LLA RRC @ 00:01:49.120

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:4

#### CRLC_Config_REQ

RRC LLA @ 00:01:49.120

Channel ID: Rb20
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:20

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC AM Channel Release REQ

LLA RLC @ 00:01:49.120

BTS unit: 1:1
Channel No: 4 Name: DCCH
CFN: 169

Message Details:

#### CRLC AM Channel Release CNF

RLC LLA @ 00:01:49.120

BTS unit: 1:1
Channel No: 4 Name: DCCH
CFN: 169

Message Details:

#### CRLC AM Channel Release REQ

LLA RLC @ 00:01:49.130

BTS unit: 1:1
Channel No: 4 Name: D_DTCH
CFN: 170

Message Details:

#### CRLC AM Channel Release CNF

RLC LLA @ 00:01:49.130

BTS unit: 1:1
Channel No: 4 Name: D_DTCH
CFN: 170

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:01:49.140

Channel ID: Rb20
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:20

#### CRLC_Config_REQ

RRC LLA @ 00:01:49.140

Channel ID: RbBcchFach
Cell ID: 6

Message Details:

CRLC_Config_REQ:

cellId:6

routingInfo:

rB_Identity:-3

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC_Config_CNF

LLA RRC @ 00:01:49.150

Channel ID: RbBcchFach
Cell ID: 6

Message Details:

CRLC_Config_CNF:

cellId:6

routingInfo:

rB_Identity:-3

#### CRLC_Config_REQ

RRC LLA @ 00:01:49.150

Channel ID: Rb0
Cell ID: 6

Message Details:

CRLC_Config_REQ:

cellId:6

routingInfo:

rB_Identity:0

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC TM Channel Release REQ

LLA RLC @ 00:01:49.150

BTS unit: 1:2
Channel No: 1 Name: BCCH
CFN: 172

Message Details:

#### CRLC TM Channel Release CNF

RLC LLA @ 00:01:49.150

BTS unit: 1:2
Channel No: 1 Name: BCCH
CFN: 172

Message Details:

#### CRLC UM Channel Release REQ

LLA RLC @ 00:01:49.160

BTS unit: 1:2
Channel No: 1 Name: CCCH
CFN: 173

Message Details:

#### CRLC UM Channel Release CNF

RLC LLA @ 00:01:49.160

BTS unit: 1:2
Channel No: 1 Name: CCCH
CFN: 173

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:01:49.170

Channel ID: Rb0
Cell ID: 6

Message Details:

CRLC_Config_CNF:

cellId:6

routingInfo:

rB_Identity:0

#### CMAC_Config_REQ

RRC LLA @ 00:01:49.170

Channel ID: PRACH#1
Cell ID: 6

Message Details:

CMAC_Config_REQ:

cellId:6

routingInfo:

physicalChannelIdentity:8

ratType:fdd

configMessage:

release:

#### CMAC Configuration REQ

LLA MAC @ 00:01:49.180

BTS unit: 1:2
Channel No: 0 Name: PRACH
CFN: 175

Message Details:

Configuration Parameters:

Number Of Transport Channels:0
Active Flag:0

Transport Format Combination Set:

Number Of Transport Format Combinations:0

#### CMAC Configuration CNF

MAC LLA @ 00:01:49.180

BTS unit: 1:2
Channel No: 0 Name: PRACH
CFN: 175

Message Details:

#### CMAC_Config_CNF

LLA RRC @ 00:01:49.190

Channel ID: PRACH#1
Cell ID: 6

Message Details:

CMAC_Config_CNF:

cellId:6

routingInfo:

physicalChannelIdentity:8

#### CPHY_TrCH_Release_REQ

RRC LLA @ 00:01:49.190

Channel ID: PRACH#1
Cell ID: 6

Message Details:

CPHY_TrCH_Release_REQ:

cellId:6

routingInfo:

physicalChannelIdentity:8

trchConfigType:

nonDch:

#### CPHY Transport Channel Release REQ

LLA PHY @ 00:01:49.190

BTS unit: 1:2
Channel No: 0 Name: PRACH
CFN: 176

Message Details:

#### CPHY Transport Channel Release CNF

PHY LLA @ 00:01:49.190

BTS unit: 1:2
Channel No: 0 Name: PRACH
CFN: 176

Message Details:

#### CPHY_TrCH_Release_CNF

LLA RRC @ 00:01:49.200

Channel ID: PRACH#1
Cell ID: 6

Message Details:

CPHY_TrCH_Release_CNF:

cellId:6

routingInfo:

physicalChannelIdentity:8

#### CPHY_RL_Release_REQ

RRC LLA @ 00:01:49.200

Channel ID: AICH#1
Cell ID: 6

Message Details:

CPHY_RL_Release_REQ:

cellId:6

routingInfo:

physicalChannelIdentity:7

#### CPHY Radio Link Release REQ

LLA PHY @ 00:01:49.210

BTS unit: 1:2
Channel No: 0 Name: AICH
CFN: 178

Message Details:

#### CPHY Radio Link Release CNF

PHY LLA @ 00:01:49.210

BTS unit: 1:2
Channel No: 0 Name: AICH
CFN: 178

Message Details:

#### CPHY_RL_Release_CNF

LLA RRC @ 00:01:49.220

Channel ID: AICH#1
Cell ID: 6

Message Details:

CPHY_RL_Release_CNF:

cellId:6

routingInfo:

physicalChannelIdentity:7

#### CPHY_RL_Release_REQ

RRC LLA @ 00:01:49.220

Channel ID: PRACH#1
Cell ID: 6

Message Details:

CPHY_RL_Release_REQ:

cellId:6

routingInfo:

physicalChannelIdentity:8

#### CPHY Radio Link Release REQ

LLA PHY @ 00:01:49.230

BTS unit: 1:2
Channel No: 0 Name: PRACH
CFN: 180

Message Details:

#### CPHY Radio Link Release CNF

PHY LLA @ 00:01:49.230

BTS unit: 1:2
Channel No: 0 Name: PRACH
CFN: 180

Message Details:

#### CPHY_RL_Release_CNF

LLA RRC @ 00:01:49.250

Channel ID: PRACH#1
Cell ID: 6

Message Details:

CPHY_RL_Release_CNF:

cellId:6

routingInfo:

physicalChannelIdentity:8

#### CRLC_Config_REQ

RRC LLA @ 00:01:49.250

Channel ID: RbPcch
Cell ID: 6

Message Details:

CRLC_Config_REQ:

cellId:6

routingInfo:

rB_Identity:-2

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC_Config_CNF

LLA RRC @ 00:01:49.260

Channel ID: RbPcch
Cell ID: 6

Message Details:

CRLC_Config_CNF:

cellId:6

routingInfo:

rB_Identity:-2

#### CMAC_Config_REQ

RRC LLA @ 00:01:49.260

Channel ID: S-CCPCH#1
Cell ID: 6

Message Details:

CMAC_Config_REQ:

cellId:6

routingInfo:

physicalChannelIdentity:5

ratType:fdd

configMessage:

release:

#### CRLC TM Channel Release REQ

LLA RLC @ 00:01:49.260

BTS unit: 1:2
Channel No: 0 Name: PCCH
CFN: 183

Message Details:

#### CRLC TM Channel Release CNF

RLC LLA @ 00:01:49.260

BTS unit: 1:2
Channel No: 0 Name: PCCH
CFN: 183

Message Details:

#### CMAC Configuration REQ

LLA MAC @ 00:01:49.280

BTS unit: 1:2
Channel No: 0 Name: S_CCPCH
CFN: 185

Message Details:

Configuration Parameters:

Number Of Transport Channels:0
Active Flag:0

Transport Format Combination Set:

Number Of Transport Format Combinations:0

#### CMAC Configuration CNF

MAC LLA @ 00:01:49.280

BTS unit: 1:2
Channel No: 0 Name: S_CCPCH
CFN: 185

Message Details:

#### CMAC_Config_CNF

LLA RRC @ 00:01:49.290

Channel ID: S-CCPCH#1
Cell ID: 6

Message Details:

CMAC_Config_CNF:

cellId:6

routingInfo:

physicalChannelIdentity:5

#### CPHY_TrCH_Release_REQ

RRC LLA @ 00:01:49.290

Channel ID: S-CCPCH#1
Cell ID: 6

Message Details:

CPHY_TrCH_Release_REQ:

cellId:6

routingInfo:

physicalChannelIdentity:5

trchConfigType:

nonDch:

#### CPHY Transport Channel Release REQ

LLA PHY @ 00:01:49.300

BTS unit: 1:2
Channel No: 0 Name: S_CCPCH
CFN: 187

Message Details:

#### CPHY Transport Channel Release CNF

PHY LLA @ 00:01:49.300

BTS unit: 1:2
Channel No: 0 Name: S_CCPCH
CFN: 187

Message Details:

#### CPHY_TrCH_Release_CNF

LLA RRC @ 00:01:49.310

Channel ID: S-CCPCH#1
Cell ID: 6

Message Details:

CPHY_TrCH_Release_CNF:

cellId:6

routingInfo:

physicalChannelIdentity:5

#### CPHY_RL_Release_REQ

RRC LLA @ 00:01:49.310

Channel ID: PICH#1
Cell ID: 6

Message Details:

CPHY_RL_Release_REQ:

cellId:6

routingInfo:

physicalChannelIdentity:6

#### CPHY Radio Link Release REQ

LLA PHY @ 00:01:49.320

BTS unit: 1:2
Channel No: 0 Name: PICH
CFN: 189

Message Details:

#### CPHY Radio Link Release CNF

PHY LLA @ 00:01:49.320

BTS unit: 1:2
Channel No: 0 Name: PICH
CFN: 189

Message Details:

#### CPHY_RL_Release_CNF

LLA RRC @ 00:01:49.330

Channel ID: PICH#1
Cell ID: 6

Message Details:

CPHY_RL_Release_CNF:

cellId:6

routingInfo:

physicalChannelIdentity:6

#### CPHY_RL_Release_REQ

RRC LLA @ 00:01:49.330

Channel ID: S-CCPCH#1
Cell ID: 6

Message Details:

CPHY_RL_Release_REQ:

cellId:6

routingInfo:

physicalChannelIdentity:5

#### CPHY Radio Link Release REQ

LLA PHY @ 00:01:49.330

BTS unit: 1:2
Channel No: 0 Name: S_CCPCH
CFN: 190

Message Details:

#### CPHY Radio Link Release CNF

PHY LLA @ 00:01:49.330

BTS unit: 1:2
Channel No: 0 Name: S_CCPCH
CFN: 190

Message Details:

#### CPHY_RL_Release_CNF

LLA RRC @ 00:01:49.340

Channel ID: S-CCPCH#1
Cell ID: 6

Message Details:

CPHY_RL_Release_CNF:

cellId:6

routingInfo:

physicalChannelIdentity:5

#### CRLC_Config_REQ

RRC LLA @ 00:01:49.340

Channel ID: RbBcch
Cell ID: 6

Message Details:

CRLC_Config_REQ:

cellId:6

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC TM Channel Release REQ

LLA RLC @ 00:01:49.350

BTS unit: 1:2
Channel No: 0 Name: BCCH
CFN: 192

Message Details:

#### CRLC TM Channel Release CNF

RLC LLA @ 00:01:49.350

BTS unit: 1:2
Channel No: 0 Name: BCCH
CFN: 192

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:01:49.360

Channel ID: RbBcch
Cell ID: 6

Message Details:

CRLC_Config_CNF:

cellId:6

routingInfo:

rB_Identity:-1

#### CMAC_Config_REQ

RRC LLA @ 00:01:49.360

Channel ID: P-CCPCH
Cell ID: 6

Message Details:

CMAC_Config_REQ:

cellId:6

routingInfo:

physicalChannelIdentity:4

ratType:fdd

configMessage:

release:

#### CMAC Configuration REQ

LLA MAC @ 00:01:49.370

BTS unit: 1:2
Channel No: 0 Name: P_CCPCH
CFN: 194

Message Details:

Configuration Parameters:

Number Of Transport Channels:0
Active Flag:0

Transport Format Combination Set:

Number Of Transport Format Combinations:0

#### CMAC Configuration CNF

MAC LLA @ 00:01:49.370

BTS unit: 1:2
Channel No: 0 Name: P_CCPCH
CFN: 194

Message Details:

#### CMAC_Config_CNF

LLA RRC @ 00:01:49.390

Channel ID: P-CCPCH
Cell ID: 6

Message Details:

CMAC_Config_CNF:

cellId:6

routingInfo:

physicalChannelIdentity:4

#### CPHY_TrCH_Release_REQ

RRC LLA @ 00:01:49.390

Channel ID: P-CCPCH
Cell ID: 6

Message Details:

CPHY_TrCH_Release_REQ:

cellId:6

routingInfo:

physicalChannelIdentity:4

trchConfigType:

nonDch:

#### CPHY_TrCH_Release_CNF

LLA RRC @ 00:01:49.400

Channel ID: P-CCPCH
Cell ID: 6

Message Details:

CPHY_TrCH_Release_CNF:

cellId:6

routingInfo:

physicalChannelIdentity:4

#### CPHY_RL_Release_REQ

RRC LLA @ 00:01:49.400

Channel ID: S-SCH
Cell ID: 6

Message Details:

CPHY_RL_Release_REQ:

cellId:6

routingInfo:

physicalChannelIdentity:2

#### CPHY Transport Channel Release REQ

LLA PHY @ 00:01:49.400

BTS unit: 1:2
Channel No: 0 Name: P_CCPCH
CFN: 197

Message Details:

#### CPHY Transport Channel Release CNF

PHY LLA @ 00:01:49.400

BTS unit: 1:2
Channel No: 0 Name: P_CCPCH
CFN: 197

Message Details:

#### CPHY Radio Link Release REQ

LLA PHY @ 00:01:49.410

BTS unit: 1:2
Channel No: 0 Name: S_SCH
CFN: 198

Message Details:

#### CPHY Radio Link Release CNF

PHY LLA @ 00:01:49.410

BTS unit: 1:2
Channel No: 0 Name: S_SCH
CFN: 198

Message Details:

#### CPHY_RL_Release_CNF

LLA RRC @ 00:01:49.420

Channel ID: S-SCH
Cell ID: 6

Message Details:

CPHY_RL_Release_CNF:

cellId:6

routingInfo:

physicalChannelIdentity:2

#### CPHY_RL_Release_REQ

RRC LLA @ 00:01:49.420

Channel ID: P-SCH
Cell ID: 6

Message Details:

CPHY_RL_Release_REQ:

cellId:6

routingInfo:

physicalChannelIdentity:1

#### CPHY Radio Link Release REQ

LLA PHY @ 00:01:49.430

BTS unit: 1:2
Channel No: 0 Name: P_SCH
CFN: 200

Message Details:

#### CPHY Radio Link Release CNF

PHY LLA @ 00:01:49.430

BTS unit: 1:2
Channel No: 0 Name: P_SCH
CFN: 200

Message Details:

#### CPHY_RL_Release_CNF

LLA RRC @ 00:01:49.440

Channel ID: P-SCH
Cell ID: 6

Message Details:

CPHY_RL_Release_CNF:

cellId:6

routingInfo:

physicalChannelIdentity:1

#### CPHY_RL_Release_REQ

RRC LLA @ 00:01:49.440

Channel ID: P-CCPCH
Cell ID: 6

Message Details:

CPHY_RL_Release_REQ:

cellId:6

routingInfo:

physicalChannelIdentity:4

#### CPHY Radio Link Release REQ

LLA PHY @ 00:01:49.440

BTS unit: 1:2
Channel No: 0 Name: P_CCPCH
CFN: 201

Message Details:

#### CPHY Radio Link Release CNF

PHY LLA @ 00:01:49.440

BTS unit: 1:2
Channel No: 0 Name: P_CCPCH
CFN: 201

Message Details:

#### CPHY_RL_Release_CNF

LLA RRC @ 00:01:49.450

Channel ID: P-CCPCH
Cell ID: 6

Message Details:

CPHY_RL_Release_CNF:

cellId:6

routingInfo:

physicalChannelIdentity:4

#### CPHY_RL_Release_REQ

RRC LLA @ 00:01:49.450

Channel ID: P-CPICH
Cell ID: 6

Message Details:

CPHY_RL_Release_REQ:

cellId:6

routingInfo:

physicalChannelIdentity:0

#### CPHY Radio Link Release REQ

LLA PHY @ 00:01:49.460

BTS unit: 1:2
Channel No: 0 Name: P_CPICH
CFN: 203

Message Details:

#### CPHY Radio Link Release CNF

PHY LLA @ 00:01:49.460

BTS unit: 1:2
Channel No: 0 Name: P_CPICH
CFN: 203

Message Details:

#### CPHY_RL_Release_CNF

LLA RRC @ 00:01:49.470

Channel ID: P-CPICH
Cell ID: 6

Message Details:

CPHY_RL_Release_CNF:

cellId:6

routingInfo:

physicalChannelIdentity:0

#### CGEN Stop REQ

RRC PHY @ 00:01:50.510

Message Details:

#### CGEN Stop CNF

PHY RRC @ 00:01:50.510

Message Details: