|  |  | RRC_wk31-Idle_Mode-tc_6_1_1_7 | Contains 6309 lines/items
| StartTimer:[1] t_Guard [300] 300 s Attach:[3] Enter Test Step tc_6_1_1_7::lt_InitVariables( )
| Attach:[12] Enter Test Step ts_RRC_InitVariables( cell_FACH )
| Attach:[1] Enter Test Step ts_AssignCN_Domain( )
| Assignment:[4] tcv_CN_Domain := ps_domain Attach:[1] Exit Test Step ts_AssignCN_Domain
Attach:[5] Enter Test Step ts_RRC_InitVariablesPS( cell_FACH )
| Attach:[1] Enter Test Step ts_InitVariables( )
| Attach:[1] Enter Test Step ts_InitVariables::lt_CalculateFrequencyInfo( )
| Attach:[10] Enter Test Step ts_InitVariables::lt_CalculateFreqMid( )
| Attach:[13] Enter Test Step ts_InitVariables::lt_CheckFreqSeperation( 10700 )
| Assignment:[30] tcv_Res := GcTRUE Attach:[13] Exit Test Step ts_InitVariables::lt_CheckFreqSeperation
Assignment:[17] tcv_FreqInfoMid := { modeSpecificInfo: [fdd: { uarfcn_UL: OMIT, uarfcn_DL: 10700 } ]} Attach:[10] Exit Test Step ts_InitVariables::lt_CalculateFreqMid
Attach:[11] Enter Test Step ts_InitVariables::lt_CalculateFreqHigh( )
| Attach:[18] Enter Test Step ts_InitVariables::lt_CheckFreqSeperation( 10837 )
| Assignment:[30] tcv_Res := GcTRUE Attach:[18] Exit Test Step ts_InitVariables::lt_CheckFreqSeperation
Assignment:[22] tcv_FreqInfoHigh := { modeSpecificInfo: [fdd: { uarfcn_UL: OMIT, uarfcn_DL: 10837 } ]} Attach:[11] Exit Test Step ts_InitVariables::lt_CalculateFreqHigh
Attach:[12] Enter Test Step ts_InitVariables::lt_CalculateFreqLow( )
| Attach:[23] Enter Test Step ts_InitVariables::lt_CheckFreqSeperation( 10563 )
| Assignment:[30] tcv_Res := GcTRUE Attach:[23] Exit Test Step ts_InitVariables::lt_CheckFreqSeperation
Assignment:[27] tcv_FreqInfoLow := { modeSpecificInfo: [fdd: { uarfcn_UL: OMIT, uarfcn_DL: 10563 } ]} Attach:[12] Exit Test Step ts_InitVariables::lt_CalculateFreqLow
Attach:[1] Exit Test Step ts_InitVariables::lt_CalculateFrequencyInfo
Attach:[2] Enter Test Step ts_InitVariables::lt_Init_SSInfo_CellA( )
| Assignment:[48] tcv_CellInfoA := (view Assignment) Attach:[2] Exit Test Step ts_InitVariables::lt_Init_SSInfo_CellA
Attach:[3] Enter Test Step ts_InitVariables::lt_Init_SSInfo_CellB( )
| Assignment:[49] tcv_CellInfoB := (view Assignment) Attach:[3] Exit Test Step ts_InitVariables::lt_Init_SSInfo_CellB
Attach:[4] Enter Test Step ts_InitVariables::lt_Init_SSInfo_CellC( )
| Assignment:[50] tcv_CellInfoC := (view Assignment) Attach:[4] Exit Test Step ts_InitVariables::lt_Init_SSInfo_CellC
Attach:[5] Enter Test Step ts_InitVariables::lt_Init_SSInfo_CellD( )
| Assignment:[51] tcv_CellInfoD := (view Assignment) Attach:[5] Exit Test Step ts_InitVariables::lt_Init_SSInfo_CellD
Attach:[6] Enter Test Step ts_InitVariables::lt_Init_SSInfo_CellE( )
| Assignment:[52] tcv_CellInfoE := (view Assignment) Attach:[6] Exit Test Step ts_InitVariables::lt_Init_SSInfo_CellE
Attach:[7] Enter Test Step ts_InitVariables::lt_Init_SSInfo_CellF( )
| Assignment:[53] tcv_CellInfoF := (view Assignment) Attach:[7] Exit Test Step ts_InitVariables::lt_Init_SSInfo_CellF
Attach:[8] Enter Test Step ts_InitVariables::lt_Init_SSInfo_CellG( )
| Assignment:[54] tcv_CellInfoG := (view Assignment) Attach:[8] Exit Test Step ts_InitVariables::lt_Init_SSInfo_CellG
Attach:[9] Enter Test Step ts_InitVariables::lt_Init_SSInfo_CellH( )
| Assignment:[55] tcv_CellInfoH := (view Assignment) Attach:[9] Exit Test Step ts_InitVariables::lt_Init_SSInfo_CellH
Attach:[1] Exit Test Step ts_InitVariables
Assignment:[2] tcv_CN_Domain := ps_domain Assignment:[2] tcv_RAB_Id := '00000101'B Assignment:[4] tcv_RRC_RAB_Type := cell_FACH_PS Attach:[5] Enter Test Step ts_RRC_InitVariablesPS::lt_RRC_InitServVarPS( cell_FACH )
| Assignment:[10] tcv_RRC_PagingCau := terminatingInteractiveCall Assignment:[10] tcv_RRC_EstCauMO := originatingInteractiveCall Assignment:[10] tcv_RRC_EstCauMT := terminatingInteractiveCall Attach:[5] Exit Test Step ts_RRC_InitVariablesPS::lt_RRC_InitServVarPS
Attach:[5] Exit Test Step ts_RRC_InitVariablesPS
Attach:[12] Exit Test Step ts_RRC_InitVariables
Attach:[13] Enter Test Step tc_6_1_1_7::lt_ITU_BandSpecificInitializing( )
| Assignment:[28] tcv_CellInfoA := (view Assignment) Assignment:[29] tcv_CellInfoD := (view Assignment) Assignment:[30] tcv_CellInfoG := (view Assignment) Attach:[13] Exit Test Step tc_6_1_1_7::lt_ITU_BandSpecificInitializing
Assignment:[14] mcc := '001'H Assignment:[14] mnc := '01F'H Assignment:[14] lac := '0001'O Assignment:[14] rac := '01'O Assignment:[14] attenuationLevel := 8 Assignment:[14] attFlag := 1 Assignment:[15] mcc := '002'H Assignment:[15] mnc := '11F'H Assignment:[15] lac := '0001'O Assignment:[15] rac := '01'O Assignment:[15] attenuationLevel := 2 Assignment:[15] attFlag := 1 Assignment:[16] mcc := '004'H Assignment:[16] mnc := '21F'H Assignment:[16] lac := '0001'O Assignment:[16] rac := '01'O Assignment:[16] attenuationLevel := 8 Assignment:[16] attFlag := 1 Attach:[3] Exit Test Step tc_6_1_1_7::lt_InitVariables
Assignment:[4] tcv_NumOfPLMN := 3 Attach:[5] Enter Test Step ts_IdleSpecificSIB_3And4Initialise( )
| Assignment:[1] q_QualMin := -24 Assignment:[1] q_QualMin := -24 Assignment:[1] q_RxlevMin := -58 Assignment:[1] q_RxlevMin := -58 Attach:[5] Exit Test Step ts_IdleSpecificSIB_3And4Initialise
Attach:[6] Enter Test Step ts_SS_CreateCellFACH( 0 )
| Attach:[1] Enter Test Step ts_SS_CellCfg( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[4] Enter Test Step ts_SS_CellCfg::lt_CelllsAlreadyStarted( 0 )
| Attach:[11] Enter Test Step ts_CountConfiguredCell( )
| Assignment:[1] tcv_NumCfgCell := 0 Attach:[2] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 0 , frequenc ...
| (view Test Step parameters) Attach:[2] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[3] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 1 , frequenc ...
| (view Test Step parameters) Attach:[3] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[4] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 2 , frequenc ...
| (view Test Step parameters) Attach:[4] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[5] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 3 , frequenc ...
| (view Test Step parameters) Attach:[5] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[6] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 4 , frequenc ...
| (view Test Step parameters) Attach:[6] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[7] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 5 , frequenc ...
| (view Test Step parameters) Attach:[7] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[8] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 4 , frequenc ...
| (view Test Step parameters) Attach:[8] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[9] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 7 , frequenc ...
| (view Test Step parameters) Attach:[9] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[11] Exit Test Step ts_CountConfiguredCell
Attach:[13] Enter Test Step ts_MM_PwrOrUSIM_Off( GcTRUE )
| Attach:[4] Enter Test Step ts_MMI_UE_SwitchOff( )
| 00:00:05.460 - Primitive: MMI_CmdReq Send event:[2] Ut ! MMI_CmdReq = PDU: { cmd: "Please switch off the UE" } 00:00:09.000 - Primitive: MMI_CmdCnf begin "ca_MMI_CmdCnf" of type MMI_CmdCnf (SEQUENCE) [UNIVERSAL 16] begin "result" of type BOOLEAN [UNIVERSAL 1] matching GcTRUE against GcTRUE end "result" of type BOOLEAN end "ca_MMI_CmdCnf" of type MMI_CmdCnf Receive event:[3] Ut ? MMI_CmdCnf = PDU: { result: GcTRUE , resultString: OMIT} Assignment:[4] tcv_UE_SwitchedOn := GcFALSE Attach:[4] Exit Test Step ts_MMI_UE_SwitchOff
Attach:[13] Exit Test Step ts_MM_PwrOrUSIM_Off
00:00:09.000 - Primitive: CPHY_Ini_REQ Send event:[15] CPHY ! CPHY_Ini_REQ = PDU: defaultRadioEnvironment 00:00:09.430 - Primitive: CPHY_Ini_CNF begin "car_IniCnf" of type CPHY_Ini_CNF (SEQUENCE) [UNIVERSAL 16] begin "confirmation" of type NULL [UNIVERSAL 5] matching NULL against NULL end "confirmation" of type NULL end "car_IniCnf" of type CPHY_Ini_CNF Receive event:[16] CPHY ? CPHY_Ini_CNF = PDU: { confirmation: NULL} Assignment:[17] tCell := 0 Attach:[4] Exit Test Step ts_SS_CellCfg::lt_CelllsAlreadyStarted
00:00:09.430 - Primitive: CPHY_Cell_Config_REQ Send event:[6] CPHY ! CPHY_Cell_Config_REQ = PDU (view PDU) 00:00:09.440 - Primitive: CPHY_Cell_Config_CNF begin "ca_CellCfgCnf" of type CPHY_Cell_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER end "ca_CellCfgCnf" of type CPHY_Cell_Config_CNF Receive event:[7] CPHY ? CPHY_Cell_Config_CNF = PDU: { cellId: 0 } Attach:[8] Enter Test Step ts_SaveCellInfo( 0 )
| Assignment:[2] tcv_CellInfoA := (view Assignment) Attach:[8] Exit Test Step ts_SaveCellInfo
Attach:[1] Exit Test Step ts_SS_CellCfg
Attach:[2] Enter Test Step ts_SS_BCH_SCH_CPICH_Cfg( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
00:00:09.440 - Primitive: CPHY_RL_Setup_REQ Send event:[3] CPHY ! CPHY_RL_Setup_REQ = PDU (view PDU) 00:00:09.470 - Primitive: CPHY_RL_Setup_CNF begin "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF Receive event:[4] CPHY ? CPHY_RL_Setup_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 0 ]} 00:00:09.470 - Primitive: CPHY_RL_Setup_REQ Send event:[5] CPHY ! CPHY_RL_Setup_REQ = PDU (view PDU) 00:00:09.490 - Primitive: CPHY_RL_Setup_CNF begin "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF Receive event:[6] CPHY ? CPHY_RL_Setup_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 1 ]} 00:00:09.490 - Primitive: CPHY_RL_Setup_REQ Send event:[7] CPHY ! CPHY_RL_Setup_REQ = PDU (view PDU) 00:00:09.500 - Primitive: CPHY_RL_Setup_CNF begin "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF Receive event:[8] CPHY ? CPHY_RL_Setup_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 2 ]} 00:00:09.500 - Primitive: CPHY_RL_Setup_REQ Send event:[9] CPHY ! CPHY_RL_Setup_REQ = PDU (view PDU) 00:00:09.520 - Primitive: CPHY_RL_Setup_CNF begin "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF Receive event:[10] CPHY ? CPHY_RL_Setup_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 4 ]} 00:00:09.520 - Primitive: CPHY_TrCH_Config_REQ Send event:[11] CPHY ! CPHY_TrCH_Config_REQ = PDU (view PDU) 00:00:09.550 - Primitive: CPHY_TrCH_Config_CNF begin "ca_TrChCfgCnf" of type CPHY_TrCH_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_TrChCfgCnf" of type CPHY_TrCH_Config_CNF Receive event:[12] CPHY ? CPHY_TrCH_Config_CNF = PDU (view PDU) 00:00:09.550 - Primitive: CMAC_Config_REQ Send event:[13] CMAC ! CMAC_Config_REQ = PDU (view PDU) 00:00:09.570 - Primitive: CMAC_Config_CNF begin "ca_CMAC_CfgCnf" of type CMAC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_CfgCnf" of type CMAC_Config_CNF Receive event:[14] CMAC ? CMAC_Config_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 4 ]} Attach:[2] Exit Test Step ts_SS_BCH_SCH_CPICH_Cfg
Attach:[3] Enter Test Step ts_CountConfiguredCell( )
| Assignment:[1] tcv_NumCfgCell := 0 Attach:[2] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 0 , frequenc ...
| (view Test Step parameters) Attach:[2] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[3] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 1 , frequenc ...
| (view Test Step parameters) Attach:[3] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[4] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 2 , frequenc ...
| (view Test Step parameters) Attach:[4] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[5] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 3 , frequenc ...
| (view Test Step parameters) Attach:[5] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[6] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 4 , frequenc ...
| (view Test Step parameters) Attach:[6] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[7] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 5 , frequenc ...
| (view Test Step parameters) Attach:[7] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[8] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 4 , frequenc ...
| (view Test Step parameters) Attach:[8] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[9] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 7 , frequenc ...
| (view Test Step parameters) Attach:[9] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[3] Exit Test Step ts_CountConfiguredCell
Attach:[5] Enter Test Step ts_SS_PCH_2FACH_CCCH_DCCH_BCCH_DTCH_Cfg( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
00:00:09.570 - Primitive: CPHY_RL_Setup_REQ Send event:[3] CPHY ! CPHY_RL_Setup_REQ = PDU (view PDU) 00:00:09.580 - Primitive: CPHY_RL_Setup_CNF begin "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 5 against 5 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF Receive event:[4] CPHY ? CPHY_RL_Setup_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 5 ]} 00:00:09.580 - Primitive: CPHY_TrCH_Config_REQ Send event:[5] CPHY ! CPHY_TrCH_Config_REQ = PDU (view PDU) 00:00:09.610 - Primitive: CPHY_TrCH_Config_CNF begin "ca_TrChCfgCnf" of type CPHY_TrCH_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 5 against 5 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_TrChCfgCnf" of type CPHY_TrCH_Config_CNF Receive event:[6] CPHY ? CPHY_TrCH_Config_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 5 ]} 00:00:09.610 - Primitive: CMAC_Config_REQ Send event:[7] CMAC ! CMAC_Config_REQ = PDU (view PDU) 00:00:09.630 - Primitive: CMAC_Config_CNF begin "ca_CMAC_CfgCnf" of type CMAC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 5 against 5 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_CfgCnf" of type CMAC_Config_CNF Receive event:[8] CMAC ? CMAC_Config_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 5 ]} 00:00:09.630 - Primitive: CPHY_RL_Setup_REQ Send event:[9] CPHY ! CPHY_RL_Setup_REQ = PDU (view PDU) 00:00:09.640 - Primitive: CPHY_RL_Setup_CNF begin "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF Receive event:[10] CPHY ? CPHY_RL_Setup_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 6 ]} Attach:[5] Exit Test Step ts_SS_PCH_2FACH_CCCH_DCCH_BCCH_DTCH_Cfg
Attach:[6] Enter Test Step ts_SS_RACH_CCCH_DCCH_DTCH_Cfg( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
00:00:09.640 - Primitive: CPHY_RL_Setup_REQ Send event:[3] CPHY ! CPHY_RL_Setup_REQ = PDU (view PDU) 00:00:09.660 - Primitive: CPHY_RL_Setup_CNF begin "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 7 against 7 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF Receive event:[4] CPHY ? CPHY_RL_Setup_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 7 ]} 00:00:09.660 - Primitive: CPHY_RL_Setup_REQ Send event:[5] CPHY ! CPHY_RL_Setup_REQ = PDU (view PDU) 00:00:09.680 - Primitive: CPHY_RL_Setup_CNF begin "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 8 against 8 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF Receive event:[6] CPHY ? CPHY_RL_Setup_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 8 ]} 00:00:09.680 - Primitive: CPHY_TrCH_Config_REQ Send event:[7] CPHY ! CPHY_TrCH_Config_REQ = PDU (view PDU) 00:00:09.720 - Primitive: CPHY_TrCH_Config_CNF begin "ca_TrChCfgCnf" of type CPHY_TrCH_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 8 against 8 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_TrChCfgCnf" of type CPHY_TrCH_Config_CNF Receive event:[8] CPHY ? CPHY_TrCH_Config_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 8 ]} 00:00:09.720 - Primitive: CMAC_Config_REQ Send event:[9] CMAC ! CMAC_Config_REQ = PDU (view PDU) 00:00:09.740 - Primitive: CMAC_Config_CNF begin "ca_CMAC_CfgCnf" of type CMAC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 8 against 8 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_CfgCnf" of type CMAC_Config_CNF Receive event:[10] CMAC ? CMAC_Config_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 8 ]} Attach:[6] Exit Test Step ts_SS_RACH_CCCH_DCCH_DTCH_Cfg
Attach:[7] Enter Test Step ts_SS_RB_BCCH_BCH_Cfg( 0 )
| 00:00:09.740 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:00:09.750 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} Attach:[7] Exit Test Step ts_SS_RB_BCCH_BCH_Cfg
Attach:[8] Enter Test Step ts_SS_RB_PCCH_Cfg( 0 )
| 00:00:09.750 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:00:09.770 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -2 against -2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -2 ]} Attach:[8] Exit Test Step ts_SS_RB_PCCH_Cfg
Attach:[9] Enter Test Step ts_SS_RB0_Cfg( 0 )
| 00:00:09.770 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:00:09.790 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: 0 ]} 00:00:09.790 - Primitive: CRLC_Config_REQ Send event:[3] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:00:09.800 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[4] CRLC ? CRLC_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: 0 ]} Attach:[9] Exit Test Step ts_SS_RB0_Cfg
Attach:[10] Enter Test Step ts_SS_RB1_ToRB4_Cfg( )
| 00:00:09.800 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:00:09.820 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 1 ]} 00:00:09.820 - Primitive: CRLC_Config_REQ Send event:[3] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:00:09.830 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[4] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 2 ]} 00:00:09.830 - Primitive: CRLC_Config_REQ Send event:[5] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:00:09.850 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[6] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 3 ]} 00:00:09.850 - Primitive: CRLC_Config_REQ Send event:[7] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:00:09.860 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[8] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 4 ]} Attach:[10] Exit Test Step ts_SS_RB1_ToRB4_Cfg
Attach:[11] Enter Test Step ts_SS_RB_BCCH_FACH_Cfg( 0 )
| 00:00:09.860 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:00:09.880 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -3 against -3 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -3 ]} Attach:[11] Exit Test Step ts_SS_RB_BCCH_FACH_Cfg
Attach:[12] Enter Test Step ts_SS_RB20_AM_PS_Cfg( 320 )
| 00:00:09.880 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:00:09.890 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 20 against 20 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 20 ]} Attach:[12] Exit Test Step ts_SS_RB20_AM_PS_Cfg
Attach:[13] Enter Test Step ts_SetCellCfg( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Assignment:[2] cellConfig := cell_FACH_NoConn Attach:[3] Enter Test Step ts_SaveCellInfo( 0 )
| Assignment:[2] tcv_CellInfoA := (view Assignment) Attach:[3] Exit Test Step ts_SaveCellInfo
Attach:[13] Exit Test Step ts_SetCellCfg
Attach:[6] Exit Test Step ts_SS_CreateCellFACH
Attach:[7] Enter Test Step ts_SendDefSysInfo_PLMN( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[2] Enter Test Step ts_UTRAN_GERAN_ParaInit( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Assignment:[3] tcv_SIB3 := (view Assignment) Assignment:[3] tcv_SIB4 := (view Assignment) Attach:[2] Exit Test Step ts_UTRAN_GERAN_ParaInit
Attach:[3] Enter Test Step ts_CellDependentPara( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Assignment:[3] cellIdentity := '0000000000000000000000000000'B Assignment:[3] cellIdentity := '0000000000000000000000000000'B Attach:[3] Exit Test Step ts_CellDependentPara
Attach:[4] Enter Test Step ts_InitializeSIB2AndSIB18( { cellId: 0 , frequenc ...
| (view Test Step parameters) Assignment:[1] tcv_SIB2 := { ura_IdentityList: [ '0000000000000001'B ] , nonCriticalExtensions: OMIT} Attach:[7] Enter Test Step ts_InitializeSIB2AndSIB18::lt_Init3PLMN( { cellId: 0 , frequenc ...
| (view Test Step parameters) Assignment:[14] tcv_SIB18 := (view Assignment) Attach:[7] Exit Test Step ts_InitializeSIB2AndSIB18::lt_Init3PLMN
Attach:[4] Exit Test Step ts_InitializeSIB2AndSIB18
Attach:[5] Enter Test Step ts_InitializeSIB11_12_SIB12_Idle( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[7] Enter Test Step ts_InitializeSIB11_12_SIB12_Idle::lt_3PLMN( 0 )
| Assignment:[27] tcv_SIB11 := (view Assignment) Assignment:[27] tcv_SIB12 := (view Assignment) Attach:[7] Exit Test Step ts_InitializeSIB11_12_SIB12_Idle::lt_3PLMN
Attach:[5] Exit Test Step ts_InitializeSIB11_12_SIB12_Idle
Assignment:[6] tcv_MIB := (view Assignment) Assignment:[6] tcv_SB1 := (view Assignment) Attach:[8] Enter Test Step ts_SendSIB1_LongNeighCellInfo( { cn_CommonGSM_MAP_NAS ...
| (view Test Step parameters) Assignment:[1] tcv_SIB1 := (view Assignment) 00:00:09.910 - Primitive: o_SIB_PER_Encoding Assignment:[1] seg1 := (view Assignment) 00:00:09.910 - Primitive: o_SIB_PER_Encoding Assignment:[1] seg2 := '00000000000000000001'B Attach:[4] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:09.910 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[4] Exit Test Step ts_Scheduling
00:00:09.930 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[5] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} 00:00:09.930 - Primitive: RLC_TR_DATA_REQ 00:00:09.930 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[6] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Assignment:[7] sysInfoType1 := 2 Attach:[8] Enter Test Step ts_ChangeMIB_ValueTag( )
| Attach:[8] Exit Test Step ts_ChangeMIB_ValueTag
Attach:[8] Exit Test Step ts_SendSIB1_LongNeighCellInfo
Attach:[9] Enter Test Step ts_SendSIB2_LongNeighCellInfo( { ura_IdentityList: [ ...
| (view Test Step parameters) Assignment:[1] tcv_SIB2 := { ura_IdentityList: [ '0000000000000001'B ] , nonCriticalExtensions: OMIT} 00:00:09.930 - Primitive: o_SIB_PER_Encoding Assignment:[1] seg1 := '00000000000000000001'B 00:00:09.930 - Primitive: o_SIB_PER_Encoding Assignment:[1] seg2 := (view Assignment) Attach:[4] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:09.930 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[4] Exit Test Step ts_Scheduling
00:00:09.940 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[5] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} 00:00:09.940 - Primitive: RLC_TR_DATA_REQ 00:00:09.940 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[6] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Assignment:[7] sysInfoType2 := 2 Attach:[8] Enter Test Step ts_ChangeMIB_ValueTag( )
| Attach:[8] Exit Test Step ts_ChangeMIB_ValueTag
Attach:[9] Exit Test Step ts_SendSIB2_LongNeighCellInfo
Attach:[10] Enter Test Step ts_SendSIB3_LongNeighCellInfo( { sib4indicator: GcTRU ...
| (view Test Step parameters) Assignment:[1] tcv_SIB3 := (view Assignment) 00:00:09.940 - Primitive: o_SIB_PER_Encoding Assignment:[1] seg1 := (view Assignment) 00:00:09.940 - Primitive: o_SIB_PER_Encoding Assignment:[1] seg2 := '100000101000000010000001'B Attach:[4] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:09.940 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[4] Exit Test Step ts_Scheduling
00:00:09.960 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[5] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} 00:00:09.960 - Primitive: RLC_TR_DATA_REQ 00:00:09.960 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[6] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Assignment:[7] sysInfoType3 := 2 Attach:[8] Enter Test Step ts_ChangeMIB_ValueTag( )
| Attach:[8] Exit Test Step ts_ChangeMIB_ValueTag
Attach:[10] Exit Test Step ts_SendSIB3_LongNeighCellInfo
Attach:[11] Enter Test Step ts_SendSIB4_LongNeighCellInfo( { cellIdentity: '00000 ...
| (view Test Step parameters) Assignment:[1] tcv_SIB4 := (view Assignment) 00:00:09.970 - Primitive: o_SIB_PER_Encoding Assignment:[1] seg1 := (view Assignment) 00:00:09.970 - Primitive: o_SIB_PER_Encoding Assignment:[1] seg2 := '100000101000000010000001'B Attach:[4] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:09.970 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[4] Exit Test Step ts_Scheduling
00:00:09.990 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[5] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} 00:00:09.990 - Primitive: RLC_TR_DATA_REQ 00:00:09.990 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[6] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Assignment:[7] sysInfoType4 := 2 Attach:[8] Enter Test Step ts_ChangeMIB_ValueTag( )
| Attach:[8] Exit Test Step ts_ChangeMIB_ValueTag
Attach:[11] Exit Test Step ts_SendSIB4_LongNeighCellInfo
Attach:[12] Enter Test Step ts_SendSIB5_LongNeighCellInfo( { sib6indicator: GcTRU ...
| (view Test Step parameters) 00:00:10.000 - Primitive: o_SIB_PER_Encoding Assignment:[1] tcv_Segs := (view Assignment) Assignment:[38] sysInfoType5 := 2 Assignment:[38] scheduling := (view Assignment) Attach:[39] Enter Test Step ts_ChangeMIB_ValueTag( )
| Attach:[39] Exit Test Step ts_ChangeMIB_ValueTag
Attach:[40] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:10.020 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[40] Exit Test Step ts_Scheduling
00:00:10.040 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[41] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} 00:00:10.040 - Primitive: RLC_TR_DATA_REQ 00:00:10.040 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[42] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[43] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:10.040 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[43] Exit Test Step ts_Scheduling
00:00:10.050 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[44] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} 00:00:10.050 - Primitive: RLC_TR_DATA_REQ 00:00:10.050 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[45] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[46] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:10.050 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[46] Exit Test Step ts_Scheduling
00:00:10.070 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[47] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} 00:00:10.070 - Primitive: RLC_TR_DATA_REQ 00:00:10.070 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[48] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[49] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:10.070 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[49] Exit Test Step ts_Scheduling
00:00:10.080 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[50] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} 00:00:10.080 - Primitive: RLC_TR_DATA_REQ 00:00:10.080 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[52] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[12] Exit Test Step ts_SendSIB5_LongNeighCellInfo
Attach:[13] Enter Test Step ts_SendSIB6_LongNeighCellInfo( { pich_PowerOffset: -5 ...
| (view Test Step parameters) 00:00:10.080 - Primitive: o_SIB_PER_Encoding Assignment:[1] tcv_Segs := (view Assignment) Assignment:[5] sysInfoType6 := 2 Assignment:[5] scheduling := { scheduling: { segCount: OMIT, sib_Pos: [rep64: 2 ], sib_PosOffsetInfo: OMIT} } Attach:[6] Enter Test Step ts_ChangeSB1_ValueTag( )
| Assignment:[2] tcv_SB1_ValueTag := 2 Assignment:[2] sysInfoTypeSB1 := 2 Assignment:[2] tcv_SB1_ValueTagChanged := GcTRUE Attach:[3] Enter Test Step ts_ChangeMIB_ValueTag( )
| Attach:[3] Exit Test Step ts_ChangeMIB_ValueTag
Attach:[6] Exit Test Step ts_ChangeSB1_ValueTag
Attach:[7] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:10.080 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[7] Exit Test Step ts_Scheduling
00:00:10.100 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[8] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} Attach:[9] Enter Test Step ts_SendSIB6_LongNeighCellInfo::lt_CompleteSIB( systemInformationBlockType6 )
| 00:00:10.100 - Primitive: RLC_TR_DATA_REQ 00:00:10.100 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[76] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[9] Exit Test Step ts_SendSIB6_LongNeighCellInfo::lt_CompleteSIB
Attach:[10] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:10.100 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[10] Exit Test Step ts_Scheduling
00:00:10.110 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[11] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} 00:00:10.110 - Primitive: RLC_TR_DATA_REQ 00:00:10.110 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[12] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[13] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:10.110 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[13] Exit Test Step ts_Scheduling
00:00:10.130 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[14] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} 00:00:10.130 - Primitive: RLC_TR_DATA_REQ 00:00:10.130 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[15] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[16] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:10.130 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[16] Exit Test Step ts_Scheduling
00:00:10.140 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[17] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} 00:00:10.140 - Primitive: RLC_TR_DATA_REQ 00:00:10.140 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[18] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[13] Exit Test Step ts_SendSIB6_LongNeighCellInfo
Attach:[14] Enter Test Step ts_SendSIB7_LongNeighCellInfo( { modeSpecificInfo: [f ...
| (view Test Step parameters) 00:00:10.140 - Primitive: o_SIB_PER_Encoding Assignment:[1] tcv_Segs := (view Assignment) Assignment:[1] tcv_SIB7 := (view Assignment) 00:00:10.160 - Primitive: o_SIB_PER_Encoding Assignment:[1] tcv_Segs_SIB12 := (view Assignment) Attach:[4] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:10.160 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[4] Exit Test Step ts_Scheduling
00:00:10.180 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[5] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} Attach:[6] Enter Test Step ts_SendSIB7_LongNeighCellInfo::lt_CompleteSIB7OrLastSIB12_CompleteSIB7( { modeSpecificInfo: [f ...
| (view Test Step parameters) 00:00:10.180 - Primitive: RLC_TR_DATA_REQ 00:00:10.180 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[36] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[6] Exit Test Step ts_SendSIB7_LongNeighCellInfo::lt_CompleteSIB7OrLastSIB12_CompleteSIB7
Attach:[7] Enter Test Step ts_SendSIB7_LongNeighCellInfo::lt_ConcatWithSIB3( { modeSpecificInfo: [f ...
| (view Test Step parameters) 00:00:10.180 - Primitive: o_SIB_PER_Encoding Assignment:[10] seg2 := (view Assignment) Attach:[13] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:10.180 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[13] Exit Test Step ts_Scheduling
00:00:10.190 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[14] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} 00:00:10.190 - Primitive: RLC_TR_DATA_REQ 00:00:10.190 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[15] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[7] Exit Test Step ts_SendSIB7_LongNeighCellInfo::lt_ConcatWithSIB3
Attach:[8] Enter Test Step ts_SendSIB7_LongNeighCellInfo::lt_ConcatWithSIB18( { modeSpecificInfo: [f ...
| (view Test Step parameters) 00:00:10.210 - Primitive: o_SIB_PER_Encoding Assignment:[16] seg2 := (view Assignment) Attach:[19] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:10.210 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[19] Exit Test Step ts_Scheduling
00:00:10.220 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[20] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} 00:00:10.220 - Primitive: RLC_TR_DATA_REQ 00:00:10.220 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[21] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[8] Exit Test Step ts_SendSIB7_LongNeighCellInfo::lt_ConcatWithSIB18
Attach:[9] Enter Test Step ts_SendSIB7_LongNeighCellInfo::lt_ConcatWithSIB4( { modeSpecificInfo: [f ...
| (view Test Step parameters) 00:00:10.220 - Primitive: o_SIB_PER_Encoding Assignment:[22] seg2 := (view Assignment) Attach:[25] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:10.220 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[25] Exit Test Step ts_Scheduling
00:00:10.240 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[26] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} 00:00:10.240 - Primitive: RLC_TR_DATA_REQ 00:00:10.240 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[27] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[9] Exit Test Step ts_SendSIB7_LongNeighCellInfo::lt_ConcatWithSIB4
Attach:[14] Exit Test Step ts_SendSIB7_LongNeighCellInfo
Attach:[15] Enter Test Step ts_SendSIB11_LongNeighCellInfo( { sib12indicator: GcTR ...
| (view Test Step parameters) 00:00:10.250 - Primitive: o_SIB_PER_Encoding Assignment:[1] tcv_Segs := (view Assignment) Assignment:[38] sysInfoType11 := 2 Assignment:[38] scheduling := (view Assignment) Attach:[39] Enter Test Step ts_ChangeSB1_ValueTag( )
| Attach:[39] Exit Test Step ts_ChangeSB1_ValueTag
Attach:[40] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:10.270 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[40] Exit Test Step ts_Scheduling
00:00:10.290 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[41] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} 00:00:10.290 - Primitive: RLC_TR_DATA_REQ 00:00:10.290 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[42] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[43] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:10.290 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[43] Exit Test Step ts_Scheduling
00:00:10.300 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[44] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} 00:00:10.300 - Primitive: RLC_TR_DATA_REQ 00:00:10.300 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[45] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[46] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:10.300 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[46] Exit Test Step ts_Scheduling
00:00:10.320 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[47] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} 00:00:10.320 - Primitive: RLC_TR_DATA_REQ 00:00:10.320 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[48] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[49] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:10.320 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[49] Exit Test Step ts_Scheduling
00:00:10.330 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[50] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} 00:00:10.330 - Primitive: RLC_TR_DATA_REQ 00:00:10.330 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[52] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[15] Exit Test Step ts_SendSIB11_LongNeighCellInfo
Attach:[16] Enter Test Step ts_SendSIB12_LongNeighCellInfo( { fach_MeasurementOcca ...
| (view Test Step parameters) 00:00:10.350 - Primitive: o_SIB_PER_Encoding Assignment:[1] tcv_Segs_SIB12 := (view Assignment) Assignment:[38] sysInfoType12 := 2 Assignment:[38] scheduling := (view Assignment) Attach:[39] Enter Test Step ts_ChangeSB1_ValueTag( )
| Attach:[39] Exit Test Step ts_ChangeSB1_ValueTag
Attach:[40] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:10.350 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[40] Exit Test Step ts_Scheduling
00:00:10.360 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[41] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} 00:00:10.360 - Primitive: RLC_TR_DATA_REQ 00:00:10.360 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[42] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[43] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:10.360 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[43] Exit Test Step ts_Scheduling
00:00:10.380 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[44] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} 00:00:10.380 - Primitive: RLC_TR_DATA_REQ 00:00:10.380 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[45] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[46] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:10.380 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[46] Exit Test Step ts_Scheduling
00:00:10.390 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[47] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} Attach:[48] Enter Test Step ts_SendSIB12_LongNeighCellInfo::lt_CompleteSIB7( { fach_MeasurementOcca ...
| (view Test Step parameters) 00:00:10.390 - Primitive: o_SIB_PER_Encoding Assignment:[74] tcv_Segs := (view Assignment) 00:00:10.390 - Primitive: RLC_TR_DATA_REQ 00:00:10.390 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[80] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[48] Exit Test Step ts_SendSIB12_LongNeighCellInfo::lt_CompleteSIB7
Attach:[49] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:10.390 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[49] Exit Test Step ts_Scheduling
00:00:10.410 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[50] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} 00:00:10.410 - Primitive: RLC_TR_DATA_REQ 00:00:10.410 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[52] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[16] Exit Test Step ts_SendSIB12_LongNeighCellInfo
Attach:[17] Enter Test Step ts_SendSIB18_LongNeighCellInfo( { idleModePLMNIdentiti ...
| (view Test Step parameters) Assignment:[1] tcv_SIB18 := (view Assignment) 00:00:10.410 - Primitive: o_SIB_PER_Encoding Assignment:[1] seg1 := (view Assignment) 00:00:10.410 - Primitive: o_SIB_PER_Encoding Assignment:[1] seg2 := '100000101000000010000001'B Attach:[4] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:10.410 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[4] Exit Test Step ts_Scheduling
00:00:10.430 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[5] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} 00:00:10.430 - Primitive: RLC_TR_DATA_REQ 00:00:10.430 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[6] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Assignment:[7] sysInfoType18 := 2 Attach:[8] Enter Test Step ts_ChangeSB1_ValueTag( )
| Attach:[8] Exit Test Step ts_ChangeSB1_ValueTag
Attach:[17] Exit Test Step ts_SendSIB18_LongNeighCellInfo
Attach:[18] Enter Test Step ts_SendSB1_LongNeighCellInfo( { sib_ReferenceList: [ ...
| (view Test Step parameters) 00:00:10.430 - Primitive: o_SIB_PER_Encoding Assignment:[1] tcv_Segs := (view Assignment) Attach:[3] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:10.430 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[3] Exit Test Step ts_Scheduling
00:00:10.440 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[4] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} Attach:[5] Enter Test Step ts_SendSB1_LongNeighCellInfo::lt_CompleteSIB( schedulingBlock1 )
| 00:00:10.440 - Primitive: RLC_TR_DATA_REQ 00:00:10.440 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[12] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[5] Exit Test Step ts_SendSB1_LongNeighCellInfo::lt_CompleteSIB
Attach:[6] Enter Test Step ts_ChangeSB1_ValueTag( )
| Attach:[6] Exit Test Step ts_ChangeSB1_ValueTag
Assignment:[7] scheduling := { scheduling: { segCount: OMIT, sib_Pos: [rep16: 1 ], sib_PosOffsetInfo: OMIT} } Assignment:[7] tcv_SB1_ValueTagChanged := GcFALSE Attach:[18] Exit Test Step ts_SendSB1_LongNeighCellInfo
Attach:[19] Enter Test Step ts_SendMIB( { mib_ValueTag: 1 , pl ...
| (view Test Step parameters) Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Assignment:[2] mcc := [ 0 , 0 , 1 ] Assignment:[2] mnc := [ 0 , 1 ] 00:00:10.440 - Primitive: o_SIB_PER_Encoding Assignment:[3] tcv_Segs := (view Assignment) Attach:[6] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:10.440 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[6] Exit Test Step ts_Scheduling
00:00:10.460 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[7] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} Attach:[8] Enter Test Step ts_SendMIB::lt_CompleteSIB( masterInformationBlock )
| 00:00:10.460 - Primitive: RLC_TR_DATA_REQ 00:00:10.460 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[13] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[8] Exit Test Step ts_SendMIB::lt_CompleteSIB
Assignment:[9] tcv_MIB_ValueTagChanged := GcFALSE Attach:[19] Exit Test Step ts_SendMIB
Attach:[20] Enter Test Step ts_SendPage1_ModifySI( 0 )
| Attach:[1] Enter Test Step ts_RRC_Delay( 5000 )
| StartTimer:[1] t_Dly [5000] 5000 ms Timed out Timer:t_Dly TimeOut:[2] t_Dly [5000] 5000 ms Attach:[1] Exit Test Step ts_RRC_Delay
Attach:[2] Enter Test Step ts_CMAC_Pag1_Cfg( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[3] Enter Test Step ts_CMAC_Pag1_Cfg::lt_CalculateDrxCycleLength( 0 )
| Assignment:[10] tcv_dRX_CycleLengthPaging := 7 Attach:[3] Exit Test Step ts_CMAC_Pag1_Cfg::lt_CalculateDrxCycleLength
00:00:15.490 - Primitive: CMAC_PAGING_Config_REQ Send event:[4] CMAC ! CMAC_PAGING_Config_REQ = PDU (view PDU) 00:00:15.500 - Primitive: CMAC_PAGING_Config_CNF begin "ca_CMAC_PagingCfgCnf" of type CMAC_PAGING_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 5 against 5 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_PagingCfgCnf" of type CMAC_PAGING_Config_CNF Receive event:[5] CMAC ? CMAC_PAGING_Config_CNF = PDU (view PDU) Attach:[2] Exit Test Step ts_CMAC_Pag1_Cfg
00:00:15.500 - Primitive: RLC_TR_DATA_REQ 00:00:15.500 - Primitive: RLC_TR_DATA_REQ: pagingType1 Send event:[3] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[4] Enter Test Step ts_SendSysInfoChangeInd_InFACHConfig( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
00:00:15.500 - Primitive: RLC_TR_DATA_REQ 00:00:15.500 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[3] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[4] Exit Test Step ts_SendSysInfoChangeInd_InFACHConfig
Attach:[20] Exit Test Step ts_SendPage1_ModifySI
Attach:[21] Enter Test Step ts_SaveBackMIB_SB1( 0 )
| Assignment:[2] tcv_MIB_CellA := (view Assignment) Assignment:[2] tcv_SB1_CellA := (view Assignment) Attach:[21] Exit Test Step ts_SaveBackMIB_SB1
Attach:[7] Exit Test Step ts_SendDefSysInfo_PLMN
Attach:[8] Enter Test Step tc_6_1_1_7::lt_LocalTest( )
| Assignment:TBS: [17] tcv_TestBody := GcTRUE Attach:[18] Enter Test Step ts_MMI_Cmd( "Please switch on the UE" )
| 00:00:15.500 - Primitive: MMI_CmdReq Send event:[1] Ut ! MMI_CmdReq = PDU: { cmd: "Please switch on the UE" } 00:00:16.610 - Primitive: MMI_CmdCnf begin "ca_MMI_CmdCnf" of type MMI_CmdCnf (SEQUENCE) [UNIVERSAL 16] begin "result" of type BOOLEAN [UNIVERSAL 1] matching GcTRUE against GcTRUE end "result" of type BOOLEAN end "ca_MMI_CmdCnf" of type MMI_CmdCnf Receive event:[2] Ut ? MMI_CmdCnf = PDU: { result: GcTRUE , resultString: OMIT} Attach:[18] Exit Test Step ts_MMI_Cmd
Assignment:[19] tcv_Use_E_PLMN := GcTRUE Assignment:[19] tcv_E_PLMN := (view Assignment) Attach:[20] Enter Test Step ts_IdleUpdated( 0 )
| Attach:[2] Enter Test Step ts_GMM_IdleUpdated( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[3] Enter Test Step ts_GMM_IdleUpdated::lt_IdleUpdated_NMO_I( 0 )
| Attach:[12] Enter Test Step ts_MMI_UE_SwitchOn( )
| 00:00:16.610 - Primitive: MMI_CmdReq Send event:[2] Ut ! MMI_CmdReq = PDU: { cmd: "Please switch on the UE" } 00:00:17.440 - Primitive: MMI_CmdCnf begin "ca_MMI_CmdCnf" of type MMI_CmdCnf (SEQUENCE) [UNIVERSAL 16] begin "result" of type BOOLEAN [UNIVERSAL 1] matching GcTRUE against GcTRUE end "result" of type BOOLEAN end "ca_MMI_CmdCnf" of type MMI_CmdCnf Receive event:[3] Ut ? MMI_CmdCnf = PDU: { result: GcTRUE , resultString: OMIT} Assignment:[4] tcv_UE_SwitchedOn := GcTRUE Attach:[12] Exit Test Step ts_MMI_UE_SwitchOn
Attach:[13] Enter Test Step ts_RRC_ConnEst( 0 )
| Attach:[1] Enter Test Step ts_SS_PrepareCellRRC_ConnEst( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[1] Exit Test Step ts_SS_PrepareCellRRC_ConnEst
Attach:[2] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[2] Exit Test Step ts_SetTmpCellInfo
Attach:[3] Enter Test Step ts_RRC_ConnEst::lt_RcvConnReq( 0 )
| 00:01:03.890 - Primitive: RLC_TR_DATA_IND: rrcConnectionRequest 00:01:03.890 - Primitive: RLC_TR_DATA_IND begin "car_RRC_ConnReq" of type RLC_TR_DATA_IND (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "tM_message" of type CHOICE [UNIVERSAL 31] begin "uL_CCCH_Message" of type UL_CCCH_Message (SEQUENCE) [UNIVERSAL 16] begin "message" of type UL_CCCH_MessageType (CHOICE) [UNIVERSAL 31] begin "rrcConnectionRequest" of type RRCConnectionRequest (SEQUENCE) [UNIVERSAL 16] begin "initialUE_Identity" of type InitialUE_Identity (CHOICE) [UNIVERSAL 31] begin InitialUE_Identity (CHOICE) [UNIVERSAL 31] end InitialUE_Identity begin InitialUE_Identity (CHOICE) [UNIVERSAL 31] begin "tmsi_and_LAI" of type TMSI_and_LAI_GSM_MAP (SEQUENCE) [UNIVERSAL 16] matching { tmsi: '00010001001000100011001101000100'B , lai: { plmn_Identity: { mcc: [ 0 , 0 , 4 ] , mnc: [ 2 , 1 ] } , lac: '0000000000000001'B } } against ? end "tmsi_and_LAI" of type TMSI_and_LAI_GSM_MAP end InitialUE_Identity matching [tmsi_and_LAI: { tmsi: '00010001001000100011001101000100'B , lai: { plmn_Identity: { mcc: [ 0 , 0 , 4 ] , mnc: [ 2 , 1 ] } , lac: '0000000000000001'B } } ] against ([imsi: ?], [tmsi_and_LAI: ?], [p_TMSI_and_RAI: ?], [imei: ?]) end "initialUE_Identity" of type InitialUE_Identity begin "establishmentCause" of type EstablishmentCause (ENUMERATED) [UNIVERSAL 10] matching registration against registration end "establishmentCause" of type EstablishmentCause begin "protocolErrorIndicator" of type ProtocolErrorIndicator (ENUMERATED) [UNIVERSAL 10] matching noError against noError end "protocolErrorIndicator" of type ProtocolErrorIndicator end "rrcConnectionRequest" of type RRCConnectionRequest end "message" of type UL_CCCH_MessageType end "uL_CCCH_Message" of type UL_CCCH_Message end "tM_message" of type CHOICE end "car_RRC_ConnReq" of type RLC_TR_DATA_IND Assignment:[7] tcv_InitialUE_Id := (view Assignment) Receive event:[7] TM ? RLC_TR_DATA_IND = PDU (view PDU) Attach:[3] Exit Test Step ts_RRC_ConnEst::lt_RcvConnReq
Attach:[4] Enter Test Step ts_RRC_ConnEst::lt_Send_ConnSetUp( 0 )
| 00:01:03.890 - Primitive: RLC_UM_DATA_REQ 00:01:03.890 - Primitive: RLC_UM_DATA_REQ: rrcConnectionSetup Send event:[11] UM ! RLC_UM_DATA_REQ = PDU (view PDU) Attach:[13] Enter Test Step ts_SetCellCfg( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Assignment:[2] cellConfig := cell_FACH Attach:[3] Enter Test Step ts_SaveCellInfo( 0 )
| Assignment:[2] tcv_CellInfoA := (view Assignment) Attach:[3] Exit Test Step ts_SaveCellInfo
Attach:[13] Exit Test Step ts_SetCellCfg
Attach:[4] Exit Test Step ts_RRC_ConnEst::lt_Send_ConnSetUp
Attach:[5] Enter Test Step ts_RRC_ReceiveConnSetupCmpl( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
StartTimer:[8] t_WaitMS [13500] 13500 ms 00:01:04.330 - Primitive: RLC_AM_DATA_IND: rrcConnectionSetupComplete 00:01:04.350 - Primitive: RLC_AM_DATA_IND begin "car_RRC_ConnSetupCmpl" of type RLC_AM_DATA_IND (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "integrityResult" of type IntegrityResult (CHOICE) [UNIVERSAL 31] matching [integrityUsed: i_pass] against ? end "integrityResult" of type IntegrityResult begin "aM_message" of type CHOICE [UNIVERSAL 31] begin "uL_DCCH_Message" of type UL_DCCH_Message (SEQUENCE) [UNIVERSAL 16] begin "message" of type UL_DCCH_MessageType (CHOICE) [UNIVERSAL 31] begin "rrcConnectionSetupComplete" of type RRCConnectionSetupComplete (SEQUENCE) [UNIVERSAL 16] begin "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier (INTEGER) [UNIVERSAL 2] matching 0 against 0 end "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier begin "startList" of type STARTList (SEQUENCEOF) [UNIVERSAL 28] matching [ { cn_DomainIdentity: ps_domain, start_Value: '00000000000000000010'B } , { cn_DomainIdentity: cs_domain, start_Value: '00000000000000000010'B } ] against ? end "startList" of type STARTList begin "ue_RadioAccessCapability" of type UE_RadioAccessCapability (SEQUENCE) [UNIVERSAL 16] matching { accessStratumReleaseIndicator: r99, pdcp_Capability: { losslessSRNS_RelocationSupport: GcTRUE , supportForRfc2507: [supported: by8192]} , rlc_Capability: { totalRLC_AM_BufferSize: kb50, maximumRLC_WindowSize: mws2047, maximumAM_EntityNumber: am6} , transportChannelCapability: { dl_TransChCapability: { maxNoBitsReceived: b5120, maxConvCodeBitsReceived: b1280, turboDecodingSupport: [supported: b5120], maxSimultaneousTransChs: e8, maxSimultaneousCCTrCH_Count: 1 , maxReceivedTransportBlocks: tb16, maxNumberOfTFC: tfc96, maxNumberOfTF: tf64} , ul_TransChCapability: { maxNoBitsTransmitted: b3840, maxConvCodeBitsTransmitted: b1280, turboEncodingSupport: [supported: b3840], maxSimultaneousTransChs: e8, modeSpecificInfo: [fdd: NULL], maxTransmittedBlocks: tb8, maxNumberOfTFC: tfc32, maxNumberOfTF: tf32} } , rf_Capability: { fddRF_Capability: { ue_PowerClass: 4 , txRxFrequencySeparation: mhz190} , tddRF_Capability: OMIT} , physicalChannelCapability: { fddPhysChCapability: { downlinkPhysChCapability: { maxNoDPCH_PDSCH_Codes: 3 , maxNoPhysChBitsReceived: b9600, supportForSF_512: GcFALSE , supportOfPDSCH: GcFALSE , simultaneousSCCPCH_DPCH_Reception: [notSupported: NULL]} , uplinkPhysChCapability: { maxNoDPDCH_BitsTransmitted: b2400, supportOfPCPCH: GcFALSE } } , tddPhysChCapability: OMIT} , ue_MultiModeRAT_Capability: { multiRAT_CapabilityList: { supportOfGSM: GcFALSE , supportOfMulticarrier: GcFALSE } , multiModeCapability: fdd} , securityCapability: { cipheringAlgorithmCap: '0000000000000001'B , integrityProtectionAlgorithmCap: '0000000000000010'B } , ue_positioning_Capability: { standaloneLocMethodsSupported: GcFALSE , ue_BasedOTDOA_Supported: GcFALSE , networkAssistedGPS_Supported: noNetworkAssistedGPS, supportForUE_GPS_TimingOfCellFrames: GcFALSE , supportForIPDL: GcFALSE } , measurementCapability: { downlinkCompressedMode: { fdd_Measurements: GcTRUE , tdd_Measurements: OMIT, gsm_Measurements: { gsm900: GcTRUE , dcs1800: GcTRUE , gsm1900: GcFALSE } , multiCarrierMeasurements: GcFALSE } , uplinkCompressedMode: { fdd_Measurements: GcTRUE , tdd_Measurements: OMIT, gsm_Measurements: { gsm900: GcTRUE , dcs1800: GcTRUE , gsm1900: GcFALSE } , multiCarrierMeasurements: GcFALSE } } } against * end "ue_RadioAccessCapability" of type UE_RadioAccessCapability end "rrcConnectionSetupComplete" of type RRCConnectionSetupComplete end "message" of type UL_DCCH_MessageType end "uL_DCCH_Message" of type UL_DCCH_Message end "aM_message" of type CHOICE end "car_RRC_ConnSetupCmpl" of type RLC_AM_DATA_IND Assignment:TSP2: [10] tcv_StartList := (view Assignment) CancelTimer:TSP2: [10] t_WaitMS [13500] 13500 ms Receive event:TSP2: [10] AM ? RLC_AM_DATA_IND = PDU (view PDU) Preliminary verdict:TSP2: [10] (PASS) Attach:[11] Enter Test Step ts_RRC_ReceiveConnSetupCmpl::lt_GetHFN( 0 )
| Assignment:[13] tcv_Count := 2 Attach:[17] Enter Test Step ts_RRC_ReceiveConnSetupCmpl::lt_FirstValue( 0 )
| Assignment:[23] start_PS := '00000000000000000010'B Attach:[17] Exit Test Step ts_RRC_ReceiveConnSetupCmpl::lt_FirstValue
Attach:[18] Enter Test Step ts_RRC_ReceiveConnSetupCmpl::lt_SecondValue( 0 )
| Assignment:[26] start_CS := '00000000000000000010'B Attach:[18] Exit Test Step ts_RRC_ReceiveConnSetupCmpl::lt_SecondValue
Attach:[11] Exit Test Step ts_RRC_ReceiveConnSetupCmpl::lt_GetHFN
Attach:[5] Exit Test Step ts_RRC_ReceiveConnSetupCmpl
Attach:[13] Exit Test Step ts_RRC_ConnEst
Attach:[15] Enter Test Step ts_GMM_IdleUpdated::lt_AttachRequest( 0 )
| Attach:[15] Exit Test Step ts_GMM_IdleUpdated::lt_AttachRequest
Attach:[15] Enter Test Step ts_GMM_IdleUpdated::lt_AttachRequest( 0 )
| Attach:[15] Exit Test Step ts_GMM_IdleUpdated::lt_AttachRequest
Attach:[15] Enter Test Step ts_GMM_IdleUpdated::lt_AttachRequest( 0 )
| Attach:[15] Exit Test Step ts_GMM_IdleUpdated::lt_AttachRequest
Attach:[15] Enter Test Step ts_GMM_IdleUpdated::lt_AttachRequest( 0 )
| Attach:[15] Exit Test Step ts_GMM_IdleUpdated::lt_AttachRequest
Attach:[15] Enter Test Step ts_GMM_IdleUpdated::lt_AttachRequest( 0 )
| Attach:[15] Exit Test Step ts_GMM_IdleUpdated::lt_AttachRequest
Attach:[15] Enter Test Step ts_GMM_IdleUpdated::lt_AttachRequest( 0 )
| Attach:[15] Exit Test Step ts_GMM_IdleUpdated::lt_AttachRequest
Attach:[15] Enter Test Step ts_GMM_IdleUpdated::lt_AttachRequest( 0 )
| Attach:[15] Exit Test Step ts_GMM_IdleUpdated::lt_AttachRequest
Attach:[15] Enter Test Step ts_GMM_IdleUpdated::lt_AttachRequest( 0 )
| Attach:[15] Exit Test Step ts_GMM_IdleUpdated::lt_AttachRequest
Attach:[15] Enter Test Step ts_GMM_IdleUpdated::lt_AttachRequest( 0 )
| Attach:[15] Exit Test Step ts_GMM_IdleUpdated::lt_AttachRequest
00:01:04.530 - Primitive: RLC_AM_DATA_IND: initialDirectTransfer 00:01:04.530 - Primitive: RRC_DATA_IND: gmm:attachRequest Attach:[15] Enter Test Step ts_GMM_IdleUpdated::lt_AttachRequest( 0 )
| begin "car_PS_InitDirectTransfer" of type RRC_DataInd (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "rB_Id" of type SS_RB_Identity (INTEGER) [UNIVERSAL 2] matching 3 against 3 end "rB_Id" of type SS_RB_Identity begin "cN_Domain" of type SS_CN_DomainIdentity (INTEGER) [UNIVERSAL 2] matching 1 against 1 end "cN_Domain" of type SS_CN_DomainIdentity begin "start" of type START_Value (BITSTRING) [UNIVERSAL 3] matching '00000000000000000010'B against ? end "start" of type START_Value begin "msg" of type ATTACHREQUEST (SEQUENCE) [UNIVERSAL 16] begin "skipIndicator" of type SkipIndicator (BITSTRING) [UNIVERSAL 3] matching '0000'B against '0000'B end "skipIndicator" of type SkipIndicator begin "gMMProtocolDiscriminator" of type ProtocolDiscriminator (BITSTRING) [UNIVERSAL 3] matching '1000'B against '1000'B end "gMMProtocolDiscriminator" of type ProtocolDiscriminator begin "msgType" of type MsgType (BITSTRING) [UNIVERSAL 3] matching '00000001'B against '00000001'B end "msgType" of type MsgType begin "msNetworkCap" of type MS_NetworkCap_lv (SEQUENCE) [UNIVERSAL 16] matching { iel: '02'O , value: 'E540'O } against ? end "msNetworkCap" of type MS_NetworkCap_lv begin "gprsCiphKeySeqNo" of type CiphKeySeqNum (SEQUENCE) [UNIVERSAL 16] begin "spare1" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against '0'B end "spare1" of type B1 begin "keySeq" of type KeySeq (BITSTRING) [UNIVERSAL 3] matching '001'B against ? end "keySeq" of type KeySeq end "gprsCiphKeySeqNo" of type CiphKeySeqNum begin "attachType" of type AttachType (SEQUENCE) [UNIVERSAL 16] begin "for" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against ? end "for" of type B1 begin "type" of type B3 (BITSTRING) [UNIVERSAL 3] matching '011'B against ? end "type" of type B3 end "attachType" of type AttachType begin "drxParameter" of type DRXparamter (SEQUENCE) [UNIVERSAL 16] matching { splitPGcycleCode: '00000111'B , cnDRXcoef: '0000'B , splitOnCCCH: '0'B , nonDRXtimer: '010'B } against ? end "drxParameter" of type DRXparamter begin "ptmsiORimsi" of type MS_Identity_lv (SEQUENCE) [UNIVERSAL 16] begin "iel" of type Length (OCTETSTRING) [UNIVERSAL 4] matching '05'O against ? end "iel" of type Length begin "iDigit1" of type B4 (BITSTRING) [UNIVERSAL 3] matching '1111'B against ? end "iDigit1" of type B4 begin "oddEvenInd" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against ? end "oddEvenInd" of type B1 begin "typeOfId" of type B3 (BITSTRING) [UNIVERSAL 3] matching '100'B against ? end "typeOfId" of type B3 begin "otherDigits" of type OCTETSTRING [UNIVERSAL 4] matching '12345678'O against ? end "otherDigits" of type OCTETSTRING end "ptmsiORimsi" of type MS_Identity_lv begin "oldRAI" of type RAI_v (SEQUENCE) [UNIVERSAL 16] begin "plmn" of type OCTETSTRING [UNIVERSAL 4] matching '00F110'O against ? end "plmn" of type OCTETSTRING begin "lac" of type OCTETSTRING [UNIVERSAL 4] matching '0001'O against ? end "lac" of type OCTETSTRING begin "rac" of type OCTETSTRING [UNIVERSAL 4] matching '05'O against ? end "rac" of type OCTETSTRING end "oldRAI" of type RAI_v begin "msRadioAccessCap" of type MSRadioAccessCap_lv (SEQUENCE) [UNIVERSAL 16] matching { iel: '0A'O , value: '14F382334C03263CA060'O } against ? end "msRadioAccessCap" of type MSRadioAccessCap_lv begin "readyTimer" of type GPRS_Timer (SEQUENCE) [UNIVERSAL 16] begin "iei" of type IEI8 (BITSTRING) [UNIVERSAL 3] matching '00010111'B against '00010111'B end "iei" of type IEI8 begin "unit" of type B3 (BITSTRING) [UNIVERSAL 3] matching '000'B against ? end "unit" of type B3 begin "value" of type B5 (BITSTRING) [UNIVERSAL 3] matching '10110'B against ? end "value" of type B5 end "readyTimer" of type GPRS_Timer end "msg" of type ATTACHREQUEST end "car_PS_InitDirectTransfer" of type RRC_DataInd Assignment:[92] tcv_TmpAttachReqPDU (view PDU) Assignment:[92] tcv_TmpB3 := '011'B Assignment:[92] tcv_Start := '00000000000000000010'B Receive event:[92] Dc ? RRC_DataInd = PDU (view PDU) Attach:[93] Enter Test Step ts_SS_SecurityDownloadStart( ps_domain )
| Assignment:[4] start_PS := '00000000000000000010'B Attach:[93] Exit Test Step ts_SS_SecurityDownloadStart
Attach:[15] Exit Test Step ts_GMM_IdleUpdated::lt_AttachRequest
Attach:[16] Enter Test Step ts_GMM_Authentication( 0 )
| Attach:[1] Enter Test Step ts_GMM_AuthenticationInit( )
| Attach:[1] Enter Test Step ts_GMM_AuthenticationInit::lt_IncrementCiphKeySeqNum( )
| Assignment:[18] tcv_PS_KeySeq := '000'B Attach:[1] Exit Test Step ts_GMM_AuthenticationInit::lt_IncrementCiphKeySeqNum
Attach:[2] Enter Test Step ts_GMM_AuthenticationInit::lt_AuthCalcAUTN( )
| Assignment:[19] tcv_AuthXDOUT := (view Assignment) Assignment:[20] tcv_AuthCDOUT := '0000000000000000000000000000000000000000000000000000000000000000'B Assignment:[21] tcv_AuthXDOUT_Half := '0101010101000100011101110110011000010001000000000011001100100010'B Assignment:[22] tcv_AuthAK := '011001100001000100000000001100110010001011011101'B Assignment:[23] tcv_AuthAUTN_1 := '011001100001000100000000001100110010001011011101'B Assignment:[24] tcv_AuthMAC := '0101010101000100011101110110011000010001000000000011001100100010'B Assignment:[25] tcv_AuthAUTN_2 := (view Assignment) Assignment:[26] tcv_AuthAUTN := (view Assignment) Attach:[2] Exit Test Step ts_GMM_AuthenticationInit::lt_AuthCalcAUTN
Attach:[3] Enter Test Step ts_GMM_AuthenticationInit::lt_AuthCalcUMTS_Others( )
| Assignment:[27] tcv_PS_AuthIK := (view Assignment) Assignment:[28] tcv_PS_AuthCK := (view Assignment) Assignment:[29] tcv_AuthXRES := (view Assignment) Attach:[3] Exit Test Step ts_GMM_AuthenticationInit::lt_AuthCalcUMTS_Others
Attach:[4] Enter Test Step ts_GMM_AuthenticationInit::lt_AuthCalcKcGSM( )
| Assignment:[30] tcv_AuthCK_1 := '0100010001110111011001100001000100000000001100110010001011011101'B Assignment:[31] tcv_AuthCK_2 := '1100110011111111111011101001100110001000101110111010101001010101'B Assignment:[32] tcv_AuthIK_1 := '0111011101100110000100010000000000110011001000101101110111001100'B Assignment:[33] tcv_AuthIK_2 := '1111111111101110100110011000100010111011101010100101010101000100'B Assignment:[34] tcv_AuthCK_XOR := '1000100010001000100010001000100010001000100010001000100010001000'B Assignment:[35] tcv_AuthIK_XOR := '1000100010001000100010001000100010001000100010001000100010001000'B Assignment:[36] tcv_AuthKcGSM := '0000000000000000000000000000000000000000000000000000000000000000'B Attach:[4] Exit Test Step ts_GMM_AuthenticationInit::lt_AuthCalcKcGSM
Attach:[1] Exit Test Step ts_GMM_AuthenticationInit
00:01:04.550 - Primitive: RRC_DATA_REQ: gmm:authenticationAndCipheringRequest 00:01:04.570 - Primitive: RLC_AM_DATA_REQ:downlinkDirectTransfer Send event:[2] Dc ! RRC_DataReq = PDU (view PDU) 00:01:05.070 - Primitive: RLC_AM_DATA_IND: uplinkDirectTransfer 00:01:05.070 - Primitive: RRC_DATA_IND: gmm:authenticationAndCipheringResponse begin "car_PS_UplinkDirectTransfer" of type RRC_DataInd (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "rB_Id" of type SS_RB_Identity (INTEGER) [UNIVERSAL 2] matching 3 against 3 end "rB_Id" of type SS_RB_Identity begin "cN_Domain" of type SS_CN_DomainIdentity (INTEGER) [UNIVERSAL 2] matching 1 against 1 end "cN_Domain" of type SS_CN_DomainIdentity begin "msg" of type AUTHENTICATIONANDCIPHERINGRESPONSE (SEQUENCE) [UNIVERSAL 16] begin "skipIndicator" of type SkipIndicator (BITSTRING) [UNIVERSAL 3] matching '0000'B against '0000'B end "skipIndicator" of type SkipIndicator begin "gMMProtocolDiscriminator" of type ProtocolDiscriminator (BITSTRING) [UNIVERSAL 3] matching '1000'B against '1000'B end "gMMProtocolDiscriminator" of type ProtocolDiscriminator begin "msgType" of type MsgType (BITSTRING) [UNIVERSAL 3] matching '00010011'B against '00010011'B end "msgType" of type MsgType begin "spare4" of type B4 (BITSTRING) [UNIVERSAL 3] matching '0000'B against '0000'B end "spare4" of type B4 begin "acRefNo" of type AC_ReferenceNumber (SEQUENCE) [UNIVERSAL 16] matching { value: '0011'B } against ? end "acRefNo" of type AC_ReferenceNumber begin "authRsp" of type AuthRsp_tv (SEQUENCE) [UNIVERSAL 16] begin "iei" of type IEI8 (BITSTRING) [UNIVERSAL 3] matching '00100010'B against '00100010'B end "iei" of type IEI8 begin "value" of type BITSTRING [UNIVERSAL 3] matching '01010101010001000111011101100110'B against ? end "value" of type BITSTRING end "authRsp" of type AuthRsp_tv begin "authRspExt" of type AuthRspExt (SEQUENCE) [UNIVERSAL 16] begin "iei" of type IEI8 (BITSTRING) [UNIVERSAL 3] matching '00101001'B against '00101001'B end "iei" of type IEI8 begin "iel" of type Length (OCTETSTRING) [UNIVERSAL 4] matching '0C'O against ? end "iel" of type Length begin "rES" of type BITSTRING [UNIVERSAL 3] matching '000100010000000000110011001000101101110111001100111111111110111010011001100010001011101110101010'B against ? end "rES" of type BITSTRING end "authRspExt" of type AuthRspExt end "msg" of type AUTHENTICATIONANDCIPHERINGRESPONSE end "car_PS_UplinkDirectTransfer" of type RRC_DataInd Assignment:[3] tcv_TmpAuthAndCiphRspPDU (view PDU) Assignment:[3] tcv_AuthRsp := '01010101010001000111011101100110'B Assignment:[3] tcv_AuthRspExt := (view Assignment) Receive event:[3] Dc ? RRC_DataInd = PDU (view PDU) Assignment:[4] tcv_Res := GcTRUE Preliminary verdict:TSP1: [6] (PASS) Attach:[16] Exit Test Step ts_GMM_Authentication
Attach:[17] Enter Test Step ts_GMM_IdleUpdated::lt_SecurityMode( 0 )
| Attach:[100] Enter Test Step ts_RRC_Security( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[2] Enter Test Step ts_RRC_Security::lt_RRC_InitVariables( 0 )
| Attach:[53] Enter Test Step ts_RRC_Security::lt_InitCipherMode( 0 )
| Assignment:[82] cs_cipheringStarted := GcFALSE Assignment:[82] ps_cipheringStarted := GcFALSE Assignment:[86] cipheringAlgorithmCapability := '0000000000000001'B Attach:[53] Exit Test Step ts_RRC_Security::lt_InitCipherMode
Attach:[54] Enter Test Step ts_RRC_Security::lt_InitIntegrity( 0 )
| Assignment:[87] recentSecureDomain := ps_domain Assignment:[92] dL_Integrity := (view Assignment) Assignment:[92] integrityStarted := GcTRUE Assignment:[92] dl_IntegrityCheckInfo := (view Assignment) Assignment:[92] tcv_Int_ModifyFlag := GcFALSE Attach:[54] Exit Test Step ts_RRC_Security::lt_InitIntegrity
Attach:[55] Enter Test Step ts_InitSystemSpecificCap( )
| Assignment:[11] tcv_UE_SystemSpecificCap := 0 Attach:[55] Exit Test Step ts_InitSystemSpecificCap
Attach:[56] Enter Test Step ts_SaveCellInfo( 0 )
| Assignment:[2] tcv_CellInfoA := (view Assignment) Attach:[56] Exit Test Step ts_SaveCellInfo
Assignment:[58] tcv_HFN := '00000000000000000000'B Assignment:[62] start_PS := '00000000000000000000'B Attach:[2] Exit Test Step ts_RRC_Security::lt_RRC_InitVariables
Attach:[3] Enter Test Step ts_SS_DownloadSecurityKey( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[13] Enter Test Step ts_SS_DownloadSecurityKey::lt_DownloadKeyCRLC( '00000000000000000000'B )
| 00:01:05.080 - Primitive: CRLC_SecurityMode_Config_REQ 00:01:05.080 - Primitive: CRLC_SecurityMode_Config_REQ Send event:[21] CRLC ! CRLC_SecurityMode_Config_REQ = PDU (view PDU) 00:01:05.100 - Primitive: CRLC_SecurityMode_Config_CNF begin "ca_CRLC_SecurityModeCfgCnf" of type CRLC_SecurityMode_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER end "ca_CRLC_SecurityModeCfgCnf" of type CRLC_SecurityMode_Config_CNF Receive event:[22] CRLC ? CRLC_SecurityMode_Config_CNF = PDU: { cellId: -1 } Attach:[13] Exit Test Step ts_SS_DownloadSecurityKey::lt_DownloadKeyCRLC
Attach:[3] Exit Test Step ts_SS_DownloadSecurityKey
Attach:[4] Enter Test Step ts_RRC_Security::lt_ActivateSecurity_DL_SS( 0 )
| Attach:[14] Enter Test Step ts_RRC_Security::lt_InitialiseRRC_MSN( 0 )
| Attach:[25] Enter Test Step ts_SetDL_RRC_MessageSN( 0 )
| 00:01:05.100 - Primitive: CRLC_SetRRC_MessageSN_REQ Send event:[1] CRLC ! CRLC_SetRRC_MessageSN_REQ = PDU (view PDU) 00:01:05.110 - Primitive: CRLC_SetRRC_MessageSN_CNF begin "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF Receive event:[2] CRLC ? CRLC_SetRRC_MessageSN_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: 0 ]} 00:01:05.110 - Primitive: CRLC_SetRRC_MessageSN_REQ Send event:[3] CRLC ! CRLC_SetRRC_MessageSN_REQ = PDU (view PDU) 00:01:05.130 - Primitive: CRLC_SetRRC_MessageSN_CNF begin "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF Receive event:[4] CRLC ? CRLC_SetRRC_MessageSN_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 1 ]} 00:01:05.130 - Primitive: CRLC_SetRRC_MessageSN_REQ Send event:[5] CRLC ! CRLC_SetRRC_MessageSN_REQ = PDU (view PDU) 00:01:05.140 - Primitive: CRLC_SetRRC_MessageSN_CNF begin "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF Receive event:[6] CRLC ? CRLC_SetRRC_MessageSN_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 2 ]} 00:01:05.140 - Primitive: CRLC_SetRRC_MessageSN_REQ Send event:[7] CRLC ! CRLC_SetRRC_MessageSN_REQ = PDU (view PDU) 00:01:05.160 - Primitive: CRLC_SetRRC_MessageSN_CNF begin "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF Receive event:[8] CRLC ? CRLC_SetRRC_MessageSN_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 3 ]} 00:01:05.160 - Primitive: CRLC_SetRRC_MessageSN_REQ Send event:[9] CRLC ! CRLC_SetRRC_MessageSN_REQ = PDU (view PDU) 00:01:05.180 - Primitive: CRLC_SetRRC_MessageSN_CNF begin "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF Receive event:[10] CRLC ? CRLC_SetRRC_MessageSN_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 4 ]} Attach:[25] Exit Test Step ts_SetDL_RRC_MessageSN
Attach:[14] Exit Test Step ts_RRC_Security::lt_InitialiseRRC_MSN
Attach:[15] Enter Test Step ts_CRLC_DL_Integrity( { integrityProtectionM ...
| (view Test Step parameters) 00:01:05.180 - Primitive: CRLC_Integrity_Activate_REQ 00:01:05.180 - Primitive: CRLC_Integrity_Activate_REQ Send event:[1] CRLC ! CRLC_Integrity_Activate_REQ = PDU (view PDU) 00:01:05.190 - Primitive: CRLC_Integrity_Activate_CNF begin "ca_CRLC_IntegrityActivateCnf" of type CRLC_Integrity_Activate_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER end "ca_CRLC_IntegrityActivateCnf" of type CRLC_Integrity_Activate_CNF Receive event:[2] CRLC ? CRLC_Integrity_Activate_CNF = PDU: { cellId: -1 } Attach:[15] Exit Test Step ts_CRLC_DL_Integrity
Attach:[4] Exit Test Step ts_RRC_Security::lt_ActivateSecurity_DL_SS
Attach:[5] Enter Test Step ts_RRC_Security::lt_RB2_UL_IntegrityActivate( 0 )
| Attach:[13] Enter Test Step ts_RB2_UL_IntegrityActivate( 0 )
| 00:01:05.190 - Primitive: CRLC_Integrity_Activate_REQ Send event:[1] CRLC ! CRLC_Integrity_Activate_REQ = PDU (view PDU) 00:01:05.210 - Primitive: CRLC_Integrity_Activate_CNF begin "ca_CRLC_IntegrityActivateCnf" of type CRLC_Integrity_Activate_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER end "ca_CRLC_IntegrityActivateCnf" of type CRLC_Integrity_Activate_CNF Receive event:[2] CRLC ? CRLC_Integrity_Activate_CNF = PDU: { cellId: -1 } Attach:[13] Exit Test Step ts_RB2_UL_IntegrityActivate
Attach:[5] Exit Test Step ts_RRC_Security::lt_RB2_UL_IntegrityActivate
Attach:[6] Enter Test Step ts_RRC_Security::lt_StartSecurity_UE( 0 )
| Attach:[27] Enter Test Step ts_RRC_Security::lt_SendSecurityModeCommand( 0 )
| 00:01:05.210 - Primitive: RLC_AM_DATA_REQ 00:01:05.210 - Primitive: RLC_AM_DATA_REQ: securityModeCommand Send event:[52] AM ! RLC_AM_DATA_REQ = PDU (view PDU) Attach:[27] Exit Test Step ts_RRC_Security::lt_SendSecurityModeCommand
00:01:05.600 - Primitive: RLC_AM_DATA_IND: securityModeComplete 00:01:05.600 - Primitive: RLC_AM_DATA_IND begin "car_RRC_SecModeCmpl" of type RLC_AM_DATA_IND (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "integrityResult" of type IntegrityResult (CHOICE) [UNIVERSAL 31] matching [integrityUsed: i_pass] against * end "integrityResult" of type IntegrityResult begin "aM_message" of type CHOICE [UNIVERSAL 31] begin "uL_DCCH_Message" of type UL_DCCH_Message (SEQUENCE) [UNIVERSAL 16] begin "integrityCheckInfo" of type IntegrityCheckInfo (SEQUENCE) [UNIVERSAL 16] matching { messageAuthenticationCode: '10001011001000110111110011100010'B , rrc_MessageSequenceNumber: 1 } against * end "integrityCheckInfo" of type IntegrityCheckInfo begin "message" of type UL_DCCH_MessageType (CHOICE) [UNIVERSAL 31] begin "securityModeComplete" of type SecurityModeComplete (SEQUENCE) [UNIVERSAL 16] begin "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier (INTEGER) [UNIVERSAL 2] matching 0 against 0 end "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier begin "ul_IntegProtActivationInfo" of type IntegrityProtActivationInfo (SEQUENCE) [UNIVERSAL 16] matching { rrc_MessageSequenceNumberList: [ 0 , 0 , 0 , 0 , 0 ] } against * end "ul_IntegProtActivationInfo" of type IntegrityProtActivationInfo end "securityModeComplete" of type SecurityModeComplete end "message" of type UL_DCCH_MessageType end "uL_DCCH_Message" of type UL_DCCH_Message end "aM_message" of type CHOICE end "car_RRC_SecModeCmpl" of type RLC_AM_DATA_IND Assignment:TSP2: [34] uL_Integrity := { rrc_MessageSequenceNumberList: [ 0 , 0 , 0 , 0 , 0 ] } Receive event:TSP2: [34] AM ? RLC_AM_DATA_IND = PDU (view PDU) Preliminary verdict:TSP2: [34] (PASS) Attach:[35] Enter Test Step ts_CRLC_UL_Integrity( { rrc_MessageSequenceNumberList: [ 0 , 0 , 0 , 0 , 0 ] } )
| 00:01:05.600 - Primitive: CRLC_Integrity_Activate_REQ Send event:[1] CRLC ! CRLC_Integrity_Activate_REQ = PDU (view PDU) 00:01:05.610 - Primitive: CRLC_Integrity_Activate_CNF begin "ca_CRLC_IntegrityActivateCnf" of type CRLC_Integrity_Activate_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER end "ca_CRLC_IntegrityActivateCnf" of type CRLC_Integrity_Activate_CNF Receive event:[2] CRLC ? CRLC_Integrity_Activate_CNF = PDU: { cellId: -1 } Attach:[35] Exit Test Step ts_CRLC_UL_Integrity
Attach:[6] Exit Test Step ts_RRC_Security::lt_StartSecurity_UE
Attach:[100] Exit Test Step ts_RRC_Security
Attach:[17] Exit Test Step ts_GMM_IdleUpdated::lt_SecurityMode
Attach:[18] Enter Test Step ts_GMM_IdleUpdated::lt_AttachAccept( 0 )
| Assignment:[102] tcv_AssignedTMSI := '11223344'O Assignment:[102] tcv_AssignedPTMSI := '12345678'O Assignment:[102] tcv_Assigned_PTMSI_Sig := 'AB1234'O 00:01:05.610 - Primitive: RRC_DATA_REQ: gmm:attachAccept 00:01:05.610 - Primitive: RLC_AM_DATA_REQ:downlinkDirectTransfer Send event:[107] Dc ! RRC_DataReq = PDU (view PDU) 00:01:05.990 - Primitive: RLC_AM_DATA_IND: uplinkDirectTransfer 00:01:05.990 - Primitive: RRC_DATA_IND: gmm:attachComplete begin "car_PS_UplinkDirectTransfer" of type RRC_DataInd (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "rB_Id" of type SS_RB_Identity (INTEGER) [UNIVERSAL 2] matching 3 against 3 end "rB_Id" of type SS_RB_Identity begin "cN_Domain" of type SS_CN_DomainIdentity (INTEGER) [UNIVERSAL 2] matching 1 against 1 end "cN_Domain" of type SS_CN_DomainIdentity begin "msg" of type ATTACHCOMPLETE (SEQUENCE) [UNIVERSAL 16] begin "skipIndicator" of type SkipIndicator (BITSTRING) [UNIVERSAL 3] matching '0000'B against '0000'B end "skipIndicator" of type SkipIndicator begin "gMMProtocolDiscriminator" of type ProtocolDiscriminator (BITSTRING) [UNIVERSAL 3] matching '1000'B against '1000'B end "gMMProtocolDiscriminator" of type ProtocolDiscriminator begin "msgType" of type MsgType (BITSTRING) [UNIVERSAL 3] matching '00000011'B against '00000011'B end "msgType" of type MsgType end "msg" of type ATTACHCOMPLETE end "car_PS_UplinkDirectTransfer" of type RRC_DataInd Receive event:[108] Dc ? RRC_DataInd = PDU (view PDU) Attach:[18] Exit Test Step ts_GMM_IdleUpdated::lt_AttachAccept
Attach:[19] Enter Test Step ts_GMM_IdleUpdated::lt_RRC_ConnRel( 0 )
| Attach:[118] Enter Test Step ts_RRC_ConnRel( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[2] Enter Test Step ts_RRC_Delay( 1000 )
| StartTimer:[1] t_Dly [5000] 1000 ms Timed out Timer:t_Dly TimeOut:[2] t_Dly [5000] 1000 ms Attach:[2] Exit Test Step ts_RRC_Delay
Attach:[3] Enter Test Step ts_RRC_ConnRel::lt_Send_RRC_ConnectionRelease( 0 )
| 00:01:07.020 - Primitive: RLC_UM_DATA_REQ 00:01:07.020 - Primitive: RLC_UM_DATA_REQ: rrcConnectionRelease Send event:[44] UM ! RLC_UM_DATA_REQ = PDU (view PDU) 00:01:07.320 - Primitive: RLC_AM_DATA_IND: rrcConnectionReleaseComplete 00:01:07.320 - Primitive: RLC_AM_DATA_IND begin "car_RRC_ConnRelCmpl" of type RLC_AM_DATA_IND (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "integrityResult" of type IntegrityResult (CHOICE) [UNIVERSAL 31] matching [integrityUsed: i_pass] against * end "integrityResult" of type IntegrityResult begin "aM_message" of type CHOICE [UNIVERSAL 31] begin "uL_DCCH_Message" of type UL_DCCH_Message (SEQUENCE) [UNIVERSAL 16] begin "integrityCheckInfo" of type IntegrityCheckInfo (SEQUENCE) [UNIVERSAL 16] matching { messageAuthenticationCode: '00011100101000000111010101000111'B , rrc_MessageSequenceNumber: 2 } against * end "integrityCheckInfo" of type IntegrityCheckInfo begin "message" of type UL_DCCH_MessageType (CHOICE) [UNIVERSAL 31] begin "rrcConnectionReleaseComplete" of type RRCConnectionReleaseComplete (SEQUENCE) [UNIVERSAL 16] begin "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier (INTEGER) [UNIVERSAL 2] matching 0 against 0 end "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier end "rrcConnectionReleaseComplete" of type RRCConnectionReleaseComplete end "message" of type UL_DCCH_MessageType end "uL_DCCH_Message" of type UL_DCCH_Message end "aM_message" of type CHOICE end "car_RRC_ConnRelCmpl" of type RLC_AM_DATA_IND Receive event:TSP2: [45] AM ? RLC_AM_DATA_IND = PDU (view PDU) Preliminary verdict:TSP2: [45] (PASS) Attach:[46] Enter Test Step ts_RRC_Delay( 1000 )
| StartTimer:[1] t_Dly [5000] 1000 ms Timed out Timer:t_Dly TimeOut:[2] t_Dly [5000] 1000 ms Attach:[46] Exit Test Step ts_RRC_Delay
Attach:[3] Exit Test Step ts_RRC_ConnRel::lt_Send_RRC_ConnectionRelease
Attach:[4] Enter Test Step ts_RRC_ConnRel::lt_RestartCRLC_ForNextConnection( 0 )
| Attach:[10] Enter Test Step ts_CRLC_RelReconfSRB( 0 )
| Attach:[1] Enter Test Step ts_CRLC_Rel( -1 )
| 00:01:08.330 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:08.350 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 1 ]} Attach:[1] Exit Test Step ts_CRLC_Rel
Attach:[2] Enter Test Step ts_CRLC_Rel( -1 )
| 00:01:08.350 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:08.360 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 2 ]} Attach:[2] Exit Test Step ts_CRLC_Rel
Attach:[3] Enter Test Step ts_CRLC_Rel( -1 )
| 00:01:08.360 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:08.380 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 3 ]} Attach:[3] Exit Test Step ts_CRLC_Rel
Attach:[4] Enter Test Step ts_CRLC_Rel( -1 )
| 00:01:08.380 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:08.390 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 4 ]} Attach:[4] Exit Test Step ts_CRLC_Rel
Attach:[5] Enter Test Step ts_SS_RB1_ToRB4_Cfg( )
| 00:01:08.390 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:08.410 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 1 ]} 00:01:08.410 - Primitive: CRLC_Config_REQ Send event:[3] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:08.430 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[4] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 2 ]} 00:01:08.430 - Primitive: CRLC_Config_REQ Send event:[5] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:08.440 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[6] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 3 ]} 00:01:08.440 - Primitive: CRLC_Config_REQ Send event:[7] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:08.460 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[8] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 4 ]} Attach:[5] Exit Test Step ts_SS_RB1_ToRB4_Cfg
Attach:[10] Exit Test Step ts_CRLC_RelReconfSRB
Attach:[11] Enter Test Step ts_SetCellCfg( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Assignment:[2] cellConfig := cell_FACH_NoConn Attach:[3] Enter Test Step ts_SaveCellInfo( 0 )
| Assignment:[2] tcv_CellInfoA := (view Assignment) Attach:[3] Exit Test Step ts_SaveCellInfo
Attach:[11] Exit Test Step ts_SetCellCfg
Attach:[4] Exit Test Step ts_RRC_ConnRel::lt_RestartCRLC_ForNextConnection
Attach:[5] Enter Test Step ts_SS_ResetSecurityKey( )
| Assignment:[1] tcv_CellIndInfo := (view Assignment) Assignment:[5] cipheringAlgorithmCapability := '0000000000000001'B Attach:[5] Exit Test Step ts_SS_ResetSecurityKey
Attach:[118] Exit Test Step ts_RRC_ConnRel
Attach:[19] Exit Test Step ts_GMM_IdleUpdated::lt_RRC_ConnRel
Attach:[3] Exit Test Step ts_GMM_IdleUpdated::lt_IdleUpdated_NMO_I
Assignment:[4] tcv_Use_E_PLMN := GcFALSE Attach:[2] Exit Test Step ts_GMM_IdleUpdated
Attach:[20] Exit Test Step ts_IdleUpdated
Attach:[21] Enter Test Step ts_SS_CreateCellFACH( 3 )
| Attach:[1] Enter Test Step ts_SS_CellCfg( 3 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 3 )
| Assignment:[8] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[4] Enter Test Step ts_SS_CellCfg::lt_CelllsAlreadyStarted( 3 )
| Attach:[11] Enter Test Step ts_CountConfiguredCell( )
| Assignment:[1] tcv_NumCfgCell := 0 Attach:[2] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 0 , frequenc ...
| (view Test Step parameters) Assignment:[11] tcv_NumCfgCell := 1 Attach:[2] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[3] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 1 , frequenc ...
| (view Test Step parameters) Attach:[3] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[4] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 2 , frequenc ...
| (view Test Step parameters) Attach:[4] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[5] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 3 , frequenc ...
| (view Test Step parameters) Attach:[5] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[6] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 4 , frequenc ...
| (view Test Step parameters) Attach:[6] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[7] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 5 , frequenc ...
| (view Test Step parameters) Attach:[7] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[8] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 4 , frequenc ...
| (view Test Step parameters) Attach:[8] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[9] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 7 , frequenc ...
| (view Test Step parameters) Attach:[9] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[11] Exit Test Step ts_CountConfiguredCell
Attach:[4] Exit Test Step ts_SS_CellCfg::lt_CelllsAlreadyStarted
00:01:08.460 - Primitive: CPHY_Cell_Config_REQ Send event:[6] CPHY ! CPHY_Cell_Config_REQ = PDU (view PDU) 00:01:08.490 - Primitive: CPHY_Cell_Config_CNF begin "ca_CellCfgCnf" of type CPHY_Cell_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER end "ca_CellCfgCnf" of type CPHY_Cell_Config_CNF Receive event:[7] CPHY ? CPHY_Cell_Config_CNF = PDU: { cellId: 3 } Attach:[8] Enter Test Step ts_SaveCellInfo( 3 )
| Assignment:[8] tcv_CellInfoD := (view Assignment) Attach:[8] Exit Test Step ts_SaveCellInfo
Attach:[1] Exit Test Step ts_SS_CellCfg
Attach:[2] Enter Test Step ts_SS_BCH_SCH_CPICH_Cfg( 3 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 3 )
| Assignment:[8] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
00:01:08.490 - Primitive: CPHY_RL_Setup_REQ Send event:[3] CPHY ! CPHY_RL_Setup_REQ = PDU (view PDU) 00:01:08.500 - Primitive: CPHY_RL_Setup_CNF begin "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF Receive event:[4] CPHY ? CPHY_RL_Setup_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 0 ]} 00:01:08.500 - Primitive: CPHY_RL_Setup_REQ Send event:[5] CPHY ! CPHY_RL_Setup_REQ = PDU (view PDU) 00:01:08.520 - Primitive: CPHY_RL_Setup_CNF begin "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF Receive event:[6] CPHY ? CPHY_RL_Setup_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 1 ]} 00:01:08.520 - Primitive: CPHY_RL_Setup_REQ Send event:[7] CPHY ! CPHY_RL_Setup_REQ = PDU (view PDU) 00:01:08.540 - Primitive: CPHY_RL_Setup_CNF begin "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF Receive event:[8] CPHY ? CPHY_RL_Setup_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 2 ]} 00:01:08.540 - Primitive: CPHY_RL_Setup_REQ Send event:[9] CPHY ! CPHY_RL_Setup_REQ = PDU (view PDU) 00:01:08.550 - Primitive: CPHY_RL_Setup_CNF begin "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF Receive event:[10] CPHY ? CPHY_RL_Setup_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 4 ]} 00:01:08.550 - Primitive: CPHY_TrCH_Config_REQ Send event:[11] CPHY ! CPHY_TrCH_Config_REQ = PDU (view PDU) 00:01:08.690 - Primitive: CPHY_TrCH_Config_CNF begin "ca_TrChCfgCnf" of type CPHY_TrCH_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_TrChCfgCnf" of type CPHY_TrCH_Config_CNF Receive event:[12] CPHY ? CPHY_TrCH_Config_CNF = PDU (view PDU) 00:01:08.690 - Primitive: CMAC_Config_REQ Send event:[13] CMAC ! CMAC_Config_REQ = PDU (view PDU) 00:01:08.710 - Primitive: CMAC_Config_CNF begin "ca_CMAC_CfgCnf" of type CMAC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_CfgCnf" of type CMAC_Config_CNF Receive event:[14] CMAC ? CMAC_Config_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 4 ]} Attach:[2] Exit Test Step ts_SS_BCH_SCH_CPICH_Cfg
Attach:[3] Enter Test Step ts_CountConfiguredCell( )
| Assignment:[1] tcv_NumCfgCell := 0 Attach:[2] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 0 , frequenc ...
| (view Test Step parameters) Assignment:[11] tcv_NumCfgCell := 1 Attach:[2] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[3] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 1 , frequenc ...
| (view Test Step parameters) Attach:[3] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[4] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 2 , frequenc ...
| (view Test Step parameters) Attach:[4] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[5] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 3 , frequenc ...
| (view Test Step parameters) Attach:[5] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[6] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 4 , frequenc ...
| (view Test Step parameters) Attach:[6] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[7] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 5 , frequenc ...
| (view Test Step parameters) Attach:[7] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[8] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 4 , frequenc ...
| (view Test Step parameters) Attach:[8] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[9] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 7 , frequenc ...
| (view Test Step parameters) Attach:[9] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[3] Exit Test Step ts_CountConfiguredCell
Attach:[15] Enter Test Step ts_SS_PCH_FACH_CCCH_Cfg( 3 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 3 )
| Assignment:[8] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
00:01:08.710 - Primitive: CPHY_RL_Setup_REQ Send event:[3] CPHY ! CPHY_RL_Setup_REQ = PDU (view PDU) 00:01:08.740 - Primitive: CPHY_RL_Setup_CNF begin "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 5 against 5 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF Receive event:[4] CPHY ? CPHY_RL_Setup_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 5 ]} 00:01:08.740 - Primitive: CPHY_TrCH_Config_REQ Send event:[5] CPHY ! CPHY_TrCH_Config_REQ = PDU (view PDU) 00:01:08.770 - Primitive: CPHY_TrCH_Config_CNF begin "ca_TrChCfgCnf" of type CPHY_TrCH_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 5 against 5 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_TrChCfgCnf" of type CPHY_TrCH_Config_CNF Receive event:[6] CPHY ? CPHY_TrCH_Config_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 5 ]} 00:01:08.770 - Primitive: CMAC_Config_REQ Send event:[7] CMAC ! CMAC_Config_REQ = PDU (view PDU) 00:01:08.790 - Primitive: CMAC_Config_CNF begin "ca_CMAC_CfgCnf" of type CMAC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 5 against 5 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_CfgCnf" of type CMAC_Config_CNF Receive event:[8] CMAC ? CMAC_Config_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 5 ]} 00:01:08.790 - Primitive: CPHY_RL_Setup_REQ Send event:[9] CPHY ! CPHY_RL_Setup_REQ = PDU (view PDU) 00:01:08.800 - Primitive: CPHY_RL_Setup_CNF begin "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF Receive event:[10] CPHY ? CPHY_RL_Setup_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 6 ]} Attach:[15] Exit Test Step ts_SS_PCH_FACH_CCCH_Cfg
Attach:[16] Enter Test Step ts_SS_RACH_CCCH_Cfg( 3 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 3 )
| Assignment:[8] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
00:01:08.800 - Primitive: CPHY_RL_Setup_REQ Send event:[3] CPHY ! CPHY_RL_Setup_REQ = PDU (view PDU) 00:01:08.830 - Primitive: CPHY_RL_Setup_CNF begin "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 7 against 7 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF Receive event:[4] CPHY ? CPHY_RL_Setup_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 7 ]} 00:01:08.830 - Primitive: CPHY_RL_Setup_REQ Send event:[5] CPHY ! CPHY_RL_Setup_REQ = PDU (view PDU) 00:01:08.850 - Primitive: CPHY_RL_Setup_CNF begin "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 8 against 8 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF Receive event:[6] CPHY ? CPHY_RL_Setup_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 8 ]} 00:01:08.850 - Primitive: CPHY_TrCH_Config_REQ Send event:[7] CPHY ! CPHY_TrCH_Config_REQ = PDU (view PDU) 00:01:08.890 - Primitive: CPHY_TrCH_Config_CNF begin "ca_TrChCfgCnf" of type CPHY_TrCH_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 8 against 8 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_TrChCfgCnf" of type CPHY_TrCH_Config_CNF Receive event:[8] CPHY ? CPHY_TrCH_Config_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 8 ]} 00:01:08.890 - Primitive: CMAC_Config_REQ Send event:[9] CMAC ! CMAC_Config_REQ = PDU (view PDU) 00:01:09.630 - Primitive: CMAC_Config_CNF begin "ca_CMAC_CfgCnf" of type CMAC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 8 against 8 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_CfgCnf" of type CMAC_Config_CNF Receive event:[10] CMAC ? CMAC_Config_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 8 ]} Attach:[16] Exit Test Step ts_SS_RACH_CCCH_Cfg
Attach:[17] Enter Test Step ts_SS_RB_BCCH_BCH_Cfg( 3 )
| 00:01:09.630 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:09.640 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} Attach:[17] Exit Test Step ts_SS_RB_BCCH_BCH_Cfg
Attach:[18] Enter Test Step ts_SS_RB_PCCH_Cfg( 3 )
| 00:01:09.640 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:09.660 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -2 against -2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -2 ]} Attach:[18] Exit Test Step ts_SS_RB_PCCH_Cfg
Attach:[19] Enter Test Step ts_SS_RB0_Cfg( 3 )
| 00:01:09.660 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:09.680 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: 0 ]} 00:01:09.680 - Primitive: CRLC_Config_REQ Send event:[3] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:09.690 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[4] CRLC ? CRLC_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: 0 ]} Attach:[19] Exit Test Step ts_SS_RB0_Cfg
Attach:[20] Enter Test Step ts_SetCellCfg( 3 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 3 )
| Assignment:[8] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Assignment:[2] cellConfig := cell_FACH_NoDedicated Attach:[3] Enter Test Step ts_SaveCellInfo( 3 )
| Assignment:[8] tcv_CellInfoD := (view Assignment) Attach:[3] Exit Test Step ts_SaveCellInfo
Attach:[20] Exit Test Step ts_SetCellCfg
Attach:[21] Exit Test Step ts_SS_CreateCellFACH
Attach:[22] Enter Test Step ts_SendDefSysInfo_PLMN( 3 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 3 )
| Assignment:[8] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[2] Enter Test Step ts_UTRAN_GERAN_ParaInit( 3 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 3 )
| Assignment:[8] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Assignment:[3] tcv_SIB3 := (view Assignment) Assignment:[3] tcv_SIB4 := (view Assignment) Attach:[2] Exit Test Step ts_UTRAN_GERAN_ParaInit
Attach:[3] Enter Test Step ts_CellDependentPara( 3 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 3 )
| Assignment:[8] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Assignment:[9] cellIdentity := '0000000000000000000000000011'B Assignment:[9] cellIdentity := '0000000000000000000000000011'B Attach:[3] Exit Test Step ts_CellDependentPara
Attach:[4] Enter Test Step ts_InitializeSIB2AndSIB18( { cellId: 3 , frequenc ...
| (view Test Step parameters) Assignment:[1] tcv_SIB2 := { ura_IdentityList: [ '0000000000000010'B ] , nonCriticalExtensions: OMIT} Attach:[7] Enter Test Step ts_InitializeSIB2AndSIB18::lt_Init3PLMN( { cellId: 3 , frequenc ...
| (view Test Step parameters) Assignment:[16] tcv_SIB18 := (view Assignment) Attach:[7] Exit Test Step ts_InitializeSIB2AndSIB18::lt_Init3PLMN
Attach:[4] Exit Test Step ts_InitializeSIB2AndSIB18
Attach:[5] Enter Test Step ts_InitializeSIB11_12_SIB12_Idle( 3 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 3 )
| Assignment:[8] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[7] Enter Test Step ts_InitializeSIB11_12_SIB12_Idle::lt_3PLMN( 3 )
| Assignment:[33] tcv_SIB11 := (view Assignment) Assignment:[33] tcv_SIB12 := (view Assignment) Attach:[7] Exit Test Step ts_InitializeSIB11_12_SIB12_Idle::lt_3PLMN
Attach:[5] Exit Test Step ts_InitializeSIB11_12_SIB12_Idle
Assignment:[6] tcv_MIB := (view Assignment) Assignment:[6] tcv_SB1 := (view Assignment) Attach:[8] Enter Test Step ts_SendSIB1_LongNeighCellInfo( { cn_CommonGSM_MAP_NAS ...
| (view Test Step parameters) Assignment:[1] tcv_SIB1 := (view Assignment) 00:01:09.710 - Primitive: o_SIB_PER_Encoding Assignment:[1] seg1 := (view Assignment) 00:01:09.710 - Primitive: o_SIB_PER_Encoding Assignment:[1] seg2 := '00000000000000000010'B Attach:[4] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:01:09.710 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[4] Exit Test Step ts_Scheduling
00:01:09.720 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[5] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} 00:01:09.720 - Primitive: RLC_TR_DATA_REQ 00:01:09.720 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[6] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Assignment:[7] sysInfoType1 := 2 Attach:[8] Enter Test Step ts_ChangeMIB_ValueTag( )
| Assignment:[2] mib_ValueTag := 2 Assignment:[2] tcv_MIB_ValueTagChanged := GcTRUE Attach:[8] Exit Test Step ts_ChangeMIB_ValueTag
Attach:[8] Exit Test Step ts_SendSIB1_LongNeighCellInfo
Attach:[9] Enter Test Step ts_SendSIB2_LongNeighCellInfo( { ura_IdentityList: [ ...
| (view Test Step parameters) Assignment:[1] tcv_SIB2 := { ura_IdentityList: [ '0000000000000010'B ] , nonCriticalExtensions: OMIT} 00:01:09.720 - Primitive: o_SIB_PER_Encoding Assignment:[1] seg1 := '00000000000000000010'B 00:01:09.720 - Primitive: o_SIB_PER_Encoding Assignment:[1] seg2 := (view Assignment) Attach:[4] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:01:09.720 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[4] Exit Test Step ts_Scheduling
00:01:09.740 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[5] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} 00:01:09.740 - Primitive: RLC_TR_DATA_REQ 00:01:09.740 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[6] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Assignment:[7] sysInfoType2 := 2 Attach:[8] Enter Test Step ts_ChangeMIB_ValueTag( )
| Attach:[8] Exit Test Step ts_ChangeMIB_ValueTag
Attach:[9] Exit Test Step ts_SendSIB2_LongNeighCellInfo
Attach:[10] Enter Test Step ts_SendSIB3_LongNeighCellInfo( { sib4indicator: GcTRU ...
| (view Test Step parameters) Assignment:[1] tcv_SIB3 := (view Assignment) 00:01:09.740 - Primitive: o_SIB_PER_Encoding Assignment:[1] seg1 := (view Assignment) 00:01:09.740 - Primitive: o_SIB_PER_Encoding Assignment:[1] seg2 := '100000101000000010000001'B Attach:[4] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:01:09.740 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[4] Exit Test Step ts_Scheduling
00:01:09.750 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[5] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} 00:01:09.750 - Primitive: RLC_TR_DATA_REQ 00:01:09.750 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[6] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Assignment:[7] sysInfoType3 := 2 Attach:[8] Enter Test Step ts_ChangeMIB_ValueTag( )
| Attach:[8] Exit Test Step ts_ChangeMIB_ValueTag
Attach:[10] Exit Test Step ts_SendSIB3_LongNeighCellInfo
Attach:[11] Enter Test Step ts_SendSIB4_LongNeighCellInfo( { cellIdentity: '00000 ...
| (view Test Step parameters) Assignment:[1] tcv_SIB4 := (view Assignment) 00:01:09.770 - Primitive: o_SIB_PER_Encoding Assignment:[1] seg1 := (view Assignment) 00:01:09.770 - Primitive: o_SIB_PER_Encoding Assignment:[1] seg2 := '100000101000000010000001'B Attach:[4] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:01:09.770 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[4] Exit Test Step ts_Scheduling
00:01:09.790 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[5] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} 00:01:09.790 - Primitive: RLC_TR_DATA_REQ 00:01:09.790 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[6] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Assignment:[7] sysInfoType4 := 2 Attach:[8] Enter Test Step ts_ChangeMIB_ValueTag( )
| Attach:[8] Exit Test Step ts_ChangeMIB_ValueTag
Attach:[11] Exit Test Step ts_SendSIB4_LongNeighCellInfo
Attach:[12] Enter Test Step ts_SendSIB5_LongNeighCellInfo( { sib6indicator: GcTRU ...
| (view Test Step parameters) 00:01:09.800 - Primitive: o_SIB_PER_Encoding Assignment:[1] tcv_Segs := (view Assignment) Assignment:[38] sysInfoType5 := 2 Assignment:[38] scheduling := (view Assignment) Attach:[39] Enter Test Step ts_ChangeMIB_ValueTag( )
| Attach:[39] Exit Test Step ts_ChangeMIB_ValueTag
Attach:[40] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:01:09.820 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[40] Exit Test Step ts_Scheduling
00:01:09.830 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[41] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} 00:01:09.830 - Primitive: RLC_TR_DATA_REQ 00:01:09.830 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[42] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[43] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:01:09.830 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[43] Exit Test Step ts_Scheduling
00:01:09.850 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[44] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} 00:01:09.850 - Primitive: RLC_TR_DATA_REQ 00:01:09.850 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[45] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[46] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:01:09.850 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[46] Exit Test Step ts_Scheduling
00:01:09.860 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[47] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} 00:01:09.860 - Primitive: RLC_TR_DATA_REQ 00:01:09.860 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[48] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[49] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:01:09.860 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[49] Exit Test Step ts_Scheduling
00:01:09.880 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[50] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} 00:01:09.880 - Primitive: RLC_TR_DATA_REQ 00:01:09.880 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[52] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[12] Exit Test Step ts_SendSIB5_LongNeighCellInfo
Attach:[13] Enter Test Step ts_SendSIB6_LongNeighCellInfo( { pich_PowerOffset: -5 ...
| (view Test Step parameters) 00:01:09.880 - Primitive: o_SIB_PER_Encoding Assignment:[1] tcv_Segs := (view Assignment) Assignment:[5] sysInfoType6 := 2 Assignment:[5] scheduling := { scheduling: { segCount: OMIT, sib_Pos: [rep64: 2 ], sib_PosOffsetInfo: OMIT} } Attach:[6] Enter Test Step ts_ChangeSB1_ValueTag( )
| Assignment:[2] tcv_SB1_ValueTag := 2 Assignment:[2] sysInfoTypeSB1 := 2 Assignment:[2] tcv_SB1_ValueTagChanged := GcTRUE Attach:[3] Enter Test Step ts_ChangeMIB_ValueTag( )
| Attach:[3] Exit Test Step ts_ChangeMIB_ValueTag
Attach:[6] Exit Test Step ts_ChangeSB1_ValueTag
Attach:[7] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:01:09.880 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[7] Exit Test Step ts_Scheduling
00:01:09.890 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[8] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} Attach:[9] Enter Test Step ts_SendSIB6_LongNeighCellInfo::lt_CompleteSIB( systemInformationBlockType6 )
| 00:01:09.890 - Primitive: RLC_TR_DATA_REQ 00:01:09.890 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[76] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[9] Exit Test Step ts_SendSIB6_LongNeighCellInfo::lt_CompleteSIB
Attach:[10] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:01:09.890 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[10] Exit Test Step ts_Scheduling
00:01:09.910 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[11] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} 00:01:09.910 - Primitive: RLC_TR_DATA_REQ 00:01:09.910 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[12] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[13] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:01:09.910 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[13] Exit Test Step ts_Scheduling
00:01:09.930 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[14] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} 00:01:09.930 - Primitive: RLC_TR_DATA_REQ 00:01:09.930 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[15] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[16] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:01:09.930 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[16] Exit Test Step ts_Scheduling
00:01:09.940 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[17] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} 00:01:09.940 - Primitive: RLC_TR_DATA_REQ 00:01:09.940 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[18] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[13] Exit Test Step ts_SendSIB6_LongNeighCellInfo
Attach:[14] Enter Test Step ts_SendSIB7_LongNeighCellInfo( { modeSpecificInfo: [f ...
| (view Test Step parameters) 00:01:09.940 - Primitive: o_SIB_PER_Encoding Assignment:[1] tcv_Segs := (view Assignment) Assignment:[1] tcv_SIB7 := (view Assignment) 00:01:09.940 - Primitive: o_SIB_PER_Encoding Assignment:[1] tcv_Segs_SIB12 := (view Assignment) Attach:[4] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:01:09.960 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[4] Exit Test Step ts_Scheduling
00:01:09.970 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[5] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} Attach:[6] Enter Test Step ts_SendSIB7_LongNeighCellInfo::lt_CompleteSIB7OrLastSIB12_CompleteSIB7( { modeSpecificInfo: [f ...
| (view Test Step parameters) 00:01:09.970 - Primitive: RLC_TR_DATA_REQ 00:01:09.970 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[36] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[6] Exit Test Step ts_SendSIB7_LongNeighCellInfo::lt_CompleteSIB7OrLastSIB12_CompleteSIB7
Attach:[7] Enter Test Step ts_SendSIB7_LongNeighCellInfo::lt_ConcatWithSIB3( { modeSpecificInfo: [f ...
| (view Test Step parameters) 00:01:09.970 - Primitive: o_SIB_PER_Encoding Assignment:[10] seg2 := (view Assignment) Attach:[13] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:01:09.970 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[13] Exit Test Step ts_Scheduling
00:01:09.990 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[14] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} 00:01:09.990 - Primitive: RLC_TR_DATA_REQ 00:01:09.990 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[15] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[7] Exit Test Step ts_SendSIB7_LongNeighCellInfo::lt_ConcatWithSIB3
Attach:[8] Enter Test Step ts_SendSIB7_LongNeighCellInfo::lt_ConcatWithSIB18( { modeSpecificInfo: [f ...
| (view Test Step parameters) 00:01:09.990 - Primitive: o_SIB_PER_Encoding Assignment:[16] seg2 := (view Assignment) Attach:[19] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:01:09.990 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[19] Exit Test Step ts_Scheduling
00:01:10.000 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[20] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} 00:01:10.000 - Primitive: RLC_TR_DATA_REQ 00:01:10.000 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[21] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[8] Exit Test Step ts_SendSIB7_LongNeighCellInfo::lt_ConcatWithSIB18
Attach:[9] Enter Test Step ts_SendSIB7_LongNeighCellInfo::lt_ConcatWithSIB4( { modeSpecificInfo: [f ...
| (view Test Step parameters) 00:01:10.000 - Primitive: o_SIB_PER_Encoding Assignment:[22] seg2 := (view Assignment) Attach:[25] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:01:10.000 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[25] Exit Test Step ts_Scheduling
00:01:10.020 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[26] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} 00:01:10.020 - Primitive: RLC_TR_DATA_REQ 00:01:10.020 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[27] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[9] Exit Test Step ts_SendSIB7_LongNeighCellInfo::lt_ConcatWithSIB4
Attach:[14] Exit Test Step ts_SendSIB7_LongNeighCellInfo
Attach:[15] Enter Test Step ts_SendSIB11_LongNeighCellInfo( { sib12indicator: GcTR ...
| (view Test Step parameters) 00:01:10.040 - Primitive: o_SIB_PER_Encoding Assignment:[1] tcv_Segs := (view Assignment) Assignment:[38] sysInfoType11 := 2 Assignment:[38] scheduling := (view Assignment) Attach:[39] Enter Test Step ts_ChangeSB1_ValueTag( )
| Attach:[39] Exit Test Step ts_ChangeSB1_ValueTag
Attach:[40] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:01:10.070 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[40] Exit Test Step ts_Scheduling
00:01:10.080 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[41] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} 00:01:10.080 - Primitive: RLC_TR_DATA_REQ 00:01:10.080 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[42] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[43] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:01:10.080 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[43] Exit Test Step ts_Scheduling
00:01:10.100 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[44] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} 00:01:10.100 - Primitive: RLC_TR_DATA_REQ 00:01:10.100 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[45] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[46] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:01:10.100 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[46] Exit Test Step ts_Scheduling
00:01:10.110 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[47] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} 00:01:10.110 - Primitive: RLC_TR_DATA_REQ 00:01:10.110 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[48] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[49] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:01:10.110 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[49] Exit Test Step ts_Scheduling
00:01:10.130 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[50] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} 00:01:10.130 - Primitive: RLC_TR_DATA_REQ 00:01:10.130 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[52] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[15] Exit Test Step ts_SendSIB11_LongNeighCellInfo
Attach:[16] Enter Test Step ts_SendSIB12_LongNeighCellInfo( { fach_MeasurementOcca ...
| (view Test Step parameters) 00:01:10.130 - Primitive: o_SIB_PER_Encoding Assignment:[1] tcv_Segs_SIB12 := (view Assignment) Assignment:[38] sysInfoType12 := 2 Assignment:[38] scheduling := (view Assignment) Attach:[39] Enter Test Step ts_ChangeSB1_ValueTag( )
| Attach:[39] Exit Test Step ts_ChangeSB1_ValueTag
Attach:[40] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:01:10.140 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[40] Exit Test Step ts_Scheduling
00:01:10.160 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[41] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} 00:01:10.160 - Primitive: RLC_TR_DATA_REQ 00:01:10.160 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[42] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[43] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:01:10.160 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[43] Exit Test Step ts_Scheduling
00:01:10.180 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[44] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} 00:01:10.180 - Primitive: RLC_TR_DATA_REQ 00:01:10.180 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[45] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[46] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:01:10.180 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[46] Exit Test Step ts_Scheduling
00:01:10.190 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[47] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} Attach:[48] Enter Test Step ts_SendSIB12_LongNeighCellInfo::lt_CompleteSIB7( { fach_MeasurementOcca ...
| (view Test Step parameters) 00:01:10.190 - Primitive: o_SIB_PER_Encoding Assignment:[74] tcv_Segs := (view Assignment) 00:01:10.190 - Primitive: RLC_TR_DATA_REQ 00:01:10.190 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[80] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[48] Exit Test Step ts_SendSIB12_LongNeighCellInfo::lt_CompleteSIB7
Attach:[49] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:01:10.190 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[49] Exit Test Step ts_Scheduling
00:01:10.210 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[50] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} 00:01:10.210 - Primitive: RLC_TR_DATA_REQ 00:01:10.210 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[52] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[16] Exit Test Step ts_SendSIB12_LongNeighCellInfo
Attach:[17] Enter Test Step ts_SendSIB18_LongNeighCellInfo( { idleModePLMNIdentiti ...
| (view Test Step parameters) Assignment:[1] tcv_SIB18 := (view Assignment) 00:01:10.210 - Primitive: o_SIB_PER_Encoding Assignment:[1] seg1 := (view Assignment) 00:01:10.210 - Primitive: o_SIB_PER_Encoding Assignment:[1] seg2 := '100000101000000010000001'B Attach:[4] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:01:10.210 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[4] Exit Test Step ts_Scheduling
00:01:10.220 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[5] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} 00:01:10.220 - Primitive: RLC_TR_DATA_REQ 00:01:10.220 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[6] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Assignment:[7] sysInfoType18 := 2 Attach:[8] Enter Test Step ts_ChangeSB1_ValueTag( )
| Attach:[8] Exit Test Step ts_ChangeSB1_ValueTag
Attach:[17] Exit Test Step ts_SendSIB18_LongNeighCellInfo
Attach:[18] Enter Test Step ts_SendSB1_LongNeighCellInfo( { sib_ReferenceList: [ ...
| (view Test Step parameters) 00:01:10.220 - Primitive: o_SIB_PER_Encoding Assignment:[1] tcv_Segs := (view Assignment) Attach:[3] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:01:10.220 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[3] Exit Test Step ts_Scheduling
00:01:10.240 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[4] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} Attach:[5] Enter Test Step ts_SendSB1_LongNeighCellInfo::lt_CompleteSIB( schedulingBlock1 )
| 00:01:10.240 - Primitive: RLC_TR_DATA_REQ 00:01:10.240 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[12] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[5] Exit Test Step ts_SendSB1_LongNeighCellInfo::lt_CompleteSIB
Attach:[6] Enter Test Step ts_ChangeSB1_ValueTag( )
| Attach:[6] Exit Test Step ts_ChangeSB1_ValueTag
Assignment:[7] scheduling := { scheduling: { segCount: OMIT, sib_Pos: [rep16: 1 ], sib_PosOffsetInfo: OMIT} } Assignment:[7] tcv_SB1_ValueTagChanged := GcFALSE Attach:[18] Exit Test Step ts_SendSB1_LongNeighCellInfo
Attach:[19] Enter Test Step ts_SendMIB( { mib_ValueTag: 2 , pl ...
| (view Test Step parameters) Attach:[1] Enter Test Step ts_SetTmpCellInfo( 3 )
| Assignment:[8] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Assignment:[2] mcc := [ 0 , 0 , 2 ] Assignment:[2] mnc := [ 1 , 1 ] 00:01:10.240 - Primitive: o_SIB_PER_Encoding Assignment:[3] tcv_Segs := (view Assignment) Attach:[6] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:01:10.250 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[6] Exit Test Step ts_Scheduling
00:01:10.270 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[7] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} Attach:[8] Enter Test Step ts_SendMIB::lt_CompleteSIB( masterInformationBlock )
| 00:01:10.270 - Primitive: RLC_TR_DATA_REQ 00:01:10.270 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[13] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[8] Exit Test Step ts_SendMIB::lt_CompleteSIB
Assignment:[9] tcv_MIB_ValueTagChanged := GcFALSE Attach:[19] Exit Test Step ts_SendMIB
Attach:[20] Enter Test Step ts_SendPage1_ModifySI( 3 )
| Attach:[1] Enter Test Step ts_RRC_Delay( 5000 )
| StartTimer:[1] t_Dly [5000] 5000 ms Timed out Timer:t_Dly TimeOut:[2] t_Dly [5000] 5000 ms Attach:[1] Exit Test Step ts_RRC_Delay
Attach:[2] Enter Test Step ts_CMAC_Pag1_Cfg( 3 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 3 )
| Assignment:[8] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[3] Enter Test Step ts_CMAC_Pag1_Cfg::lt_CalculateDrxCycleLength( 3 )
| Assignment:[10] tcv_dRX_CycleLengthPaging := 7 Attach:[3] Exit Test Step ts_CMAC_Pag1_Cfg::lt_CalculateDrxCycleLength
00:01:15.290 - Primitive: CMAC_PAGING_Config_REQ Send event:[4] CMAC ! CMAC_PAGING_Config_REQ = PDU (view PDU) 00:01:15.300 - Primitive: CMAC_PAGING_Config_CNF begin "ca_CMAC_PagingCfgCnf" of type CMAC_PAGING_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 5 against 5 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_PagingCfgCnf" of type CMAC_PAGING_Config_CNF Receive event:[5] CMAC ? CMAC_PAGING_Config_CNF = PDU (view PDU) Attach:[2] Exit Test Step ts_CMAC_Pag1_Cfg
00:01:15.300 - Primitive: RLC_TR_DATA_REQ 00:01:15.300 - Primitive: RLC_TR_DATA_REQ: pagingType1 Send event:[3] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[4] Enter Test Step ts_SendSysInfoChangeInd_InFACHConfig( 3 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 3 )
| Assignment:[8] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[4] Exit Test Step ts_SendSysInfoChangeInd_InFACHConfig
Attach:[20] Exit Test Step ts_SendPage1_ModifySI
Attach:[21] Enter Test Step ts_SaveBackMIB_SB1( 3 )
| Assignment:[8] tcv_MIB_CellD := (view Assignment) Assignment:[8] tcv_SB1_CellD := (view Assignment) Attach:[21] Exit Test Step ts_SaveBackMIB_SB1
Attach:[22] Exit Test Step ts_SendDefSysInfo_PLMN
Attach:[23] Enter Test Step ts_SS_CreateCellFACH( 6 )
| Attach:[1] Enter Test Step ts_SS_CellCfg( 6 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 6 )
| Assignment:[14] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[4] Enter Test Step ts_SS_CellCfg::lt_CelllsAlreadyStarted( 6 )
| Attach:[11] Enter Test Step ts_CountConfiguredCell( )
| Assignment:[1] tcv_NumCfgCell := 0 Attach:[2] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 0 , frequenc ...
| (view Test Step parameters) Assignment:[11] tcv_NumCfgCell := 1 Attach:[2] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[3] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 1 , frequenc ...
| (view Test Step parameters) Attach:[3] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[4] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 2 , frequenc ...
| (view Test Step parameters) Attach:[4] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[5] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 3 , frequenc ...
| (view Test Step parameters) Assignment:[11] tcv_NumCfgCell := 2 Attach:[5] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[6] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 4 , frequenc ...
| (view Test Step parameters) Attach:[6] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[7] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 5 , frequenc ...
| (view Test Step parameters) Attach:[7] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[8] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 4 , frequenc ...
| (view Test Step parameters) Attach:[8] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[9] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 7 , frequenc ...
| (view Test Step parameters) Attach:[9] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[11] Exit Test Step ts_CountConfiguredCell
Attach:[4] Exit Test Step ts_SS_CellCfg::lt_CelllsAlreadyStarted
00:01:15.300 - Primitive: CPHY_Cell_Config_REQ Send event:[6] CPHY ! CPHY_Cell_Config_REQ = PDU (view PDU) 00:01:15.330 - Primitive: CPHY_Cell_Config_CNF begin "ca_CellCfgCnf" of type CPHY_Cell_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "cellId" of type INTEGER end "ca_CellCfgCnf" of type CPHY_Cell_Config_CNF Receive event:[7] CPHY ? CPHY_Cell_Config_CNF = PDU: { cellId: 6 } Attach:[8] Enter Test Step ts_SaveCellInfo( 6 )
| Assignment:[14] tcv_CellInfoG := (view Assignment) Attach:[8] Exit Test Step ts_SaveCellInfo
Attach:[1] Exit Test Step ts_SS_CellCfg
Attach:[2] Enter Test Step ts_SS_BCH_SCH_CPICH_Cfg( 6 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 6 )
| Assignment:[14] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
00:01:15.330 - Primitive: CPHY_RL_Setup_REQ Send event:[3] CPHY ! CPHY_RL_Setup_REQ = PDU (view PDU) 00:01:15.350 - Primitive: CPHY_RL_Setup_CNF begin "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF Receive event:[4] CPHY ? CPHY_RL_Setup_CNF = PDU: { cellId: 6 , routingInfo: [physicalChannelIdentity: 0 ]} 00:01:15.350 - Primitive: CPHY_RL_Setup_REQ Send event:[5] CPHY ! CPHY_RL_Setup_REQ = PDU (view PDU) 00:01:15.360 - Primitive: CPHY_RL_Setup_CNF begin "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF Receive event:[6] CPHY ? CPHY_RL_Setup_CNF = PDU: { cellId: 6 , routingInfo: [physicalChannelIdentity: 1 ]} 00:01:15.360 - Primitive: CPHY_RL_Setup_REQ Send event:[7] CPHY ! CPHY_RL_Setup_REQ = PDU (view PDU) 00:01:15.380 - Primitive: CPHY_RL_Setup_CNF begin "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF Receive event:[8] CPHY ? CPHY_RL_Setup_CNF = PDU: { cellId: 6 , routingInfo: [physicalChannelIdentity: 2 ]} 00:01:15.380 - Primitive: CPHY_RL_Setup_REQ Send event:[9] CPHY ! CPHY_RL_Setup_REQ = PDU (view PDU) 00:01:15.390 - Primitive: CPHY_RL_Setup_CNF begin "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF Receive event:[10] CPHY ? CPHY_RL_Setup_CNF = PDU: { cellId: 6 , routingInfo: [physicalChannelIdentity: 4 ]} 00:01:15.390 - Primitive: CPHY_TrCH_Config_REQ Send event:[11] CPHY ! CPHY_TrCH_Config_REQ = PDU (view PDU) 00:01:15.430 - Primitive: CPHY_TrCH_Config_CNF begin "ca_TrChCfgCnf" of type CPHY_TrCH_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_TrChCfgCnf" of type CPHY_TrCH_Config_CNF Receive event:[12] CPHY ? CPHY_TrCH_Config_CNF = PDU (view PDU) 00:01:15.430 - Primitive: CMAC_Config_REQ Send event:[13] CMAC ! CMAC_Config_REQ = PDU (view PDU) 00:01:15.460 - Primitive: CMAC_Config_CNF begin "ca_CMAC_CfgCnf" of type CMAC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_CfgCnf" of type CMAC_Config_CNF Receive event:[14] CMAC ? CMAC_Config_CNF = PDU: { cellId: 6 , routingInfo: [physicalChannelIdentity: 4 ]} Attach:[2] Exit Test Step ts_SS_BCH_SCH_CPICH_Cfg
Attach:[3] Enter Test Step ts_CountConfiguredCell( )
| Assignment:[1] tcv_NumCfgCell := 0 Attach:[2] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 0 , frequenc ...
| (view Test Step parameters) Assignment:[11] tcv_NumCfgCell := 1 Attach:[2] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[3] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 1 , frequenc ...
| (view Test Step parameters) Attach:[3] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[4] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 2 , frequenc ...
| (view Test Step parameters) Attach:[4] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[5] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 3 , frequenc ...
| (view Test Step parameters) Assignment:[11] tcv_NumCfgCell := 2 Attach:[5] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[6] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 4 , frequenc ...
| (view Test Step parameters) Attach:[6] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[7] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 5 , frequenc ...
| (view Test Step parameters) Attach:[7] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[8] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 4 , frequenc ...
| (view Test Step parameters) Attach:[8] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[9] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 7 , frequenc ...
| (view Test Step parameters) Attach:[9] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[3] Exit Test Step ts_CountConfiguredCell
Attach:[15] Enter Test Step ts_SS_PCH_FACH_CCCH_Cfg( 6 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 6 )
| Assignment:[14] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
00:01:15.460 - Primitive: CPHY_RL_Setup_REQ Send event:[3] CPHY ! CPHY_RL_Setup_REQ = PDU (view PDU) 00:01:15.470 - Primitive: CPHY_RL_Setup_CNF begin "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 5 against 5 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF Receive event:[4] CPHY ? CPHY_RL_Setup_CNF = PDU: { cellId: 6 , routingInfo: [physicalChannelIdentity: 5 ]} 00:01:15.470 - Primitive: CPHY_TrCH_Config_REQ Send event:[5] CPHY ! CPHY_TrCH_Config_REQ = PDU (view PDU) 00:01:15.490 - Primitive: CPHY_TrCH_Config_CNF begin "ca_TrChCfgCnf" of type CPHY_TrCH_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 5 against 5 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_TrChCfgCnf" of type CPHY_TrCH_Config_CNF Receive event:[6] CPHY ? CPHY_TrCH_Config_CNF = PDU: { cellId: 6 , routingInfo: [physicalChannelIdentity: 5 ]} 00:01:15.490 - Primitive: CMAC_Config_REQ Send event:[7] CMAC ! CMAC_Config_REQ = PDU (view PDU) 00:01:15.500 - Primitive: CMAC_Config_CNF begin "ca_CMAC_CfgCnf" of type CMAC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 5 against 5 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_CfgCnf" of type CMAC_Config_CNF Receive event:[8] CMAC ? CMAC_Config_CNF = PDU: { cellId: 6 , routingInfo: [physicalChannelIdentity: 5 ]} 00:01:15.500 - Primitive: CPHY_RL_Setup_REQ Send event:[9] CPHY ! CPHY_RL_Setup_REQ = PDU (view PDU) 00:01:15.520 - Primitive: CPHY_RL_Setup_CNF begin "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF Receive event:[10] CPHY ? CPHY_RL_Setup_CNF = PDU: { cellId: 6 , routingInfo: [physicalChannelIdentity: 6 ]} Attach:[15] Exit Test Step ts_SS_PCH_FACH_CCCH_Cfg
Attach:[16] Enter Test Step ts_SS_RACH_CCCH_Cfg( 6 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 6 )
| Assignment:[14] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
00:01:15.520 - Primitive: CPHY_RL_Setup_REQ Send event:[3] CPHY ! CPHY_RL_Setup_REQ = PDU (view PDU) 00:01:15.540 - Primitive: CPHY_RL_Setup_CNF begin "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 7 against 7 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF Receive event:[4] CPHY ? CPHY_RL_Setup_CNF = PDU: { cellId: 6 , routingInfo: [physicalChannelIdentity: 7 ]} 00:01:15.540 - Primitive: CPHY_RL_Setup_REQ Send event:[5] CPHY ! CPHY_RL_Setup_REQ = PDU (view PDU) 00:01:15.550 - Primitive: CPHY_RL_Setup_CNF begin "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 8 against 8 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF Receive event:[6] CPHY ? CPHY_RL_Setup_CNF = PDU: { cellId: 6 , routingInfo: [physicalChannelIdentity: 8 ]} 00:01:15.550 - Primitive: CPHY_TrCH_Config_REQ Send event:[7] CPHY ! CPHY_TrCH_Config_REQ = PDU (view PDU) 00:01:15.600 - Primitive: CPHY_TrCH_Config_CNF begin "ca_TrChCfgCnf" of type CPHY_TrCH_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 8 against 8 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_TrChCfgCnf" of type CPHY_TrCH_Config_CNF Receive event:[8] CPHY ? CPHY_TrCH_Config_CNF = PDU: { cellId: 6 , routingInfo: [physicalChannelIdentity: 8 ]} 00:01:15.600 - Primitive: CMAC_Config_REQ Send event:[9] CMAC ! CMAC_Config_REQ = PDU (view PDU) 00:01:15.630 - Primitive: CMAC_Config_CNF begin "ca_CMAC_CfgCnf" of type CMAC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 8 against 8 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_CfgCnf" of type CMAC_Config_CNF Receive event:[10] CMAC ? CMAC_Config_CNF = PDU: { cellId: 6 , routingInfo: [physicalChannelIdentity: 8 ]} Attach:[16] Exit Test Step ts_SS_RACH_CCCH_Cfg
Attach:[17] Enter Test Step ts_SS_RB_BCCH_BCH_Cfg( 6 )
| 00:01:15.630 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:15.640 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: 6 , routingInfo: [rB_Identity: -1 ]} Attach:[17] Exit Test Step ts_SS_RB_BCCH_BCH_Cfg
Attach:[18] Enter Test Step ts_SS_RB_PCCH_Cfg( 6 )
| 00:01:15.640 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:15.660 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -2 against -2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: 6 , routingInfo: [rB_Identity: -2 ]} Attach:[18] Exit Test Step ts_SS_RB_PCCH_Cfg
Attach:[19] Enter Test Step ts_SS_RB0_Cfg( 6 )
| 00:01:15.660 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:15.680 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: 6 , routingInfo: [rB_Identity: 0 ]} 00:01:15.680 - Primitive: CRLC_Config_REQ Send event:[3] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:15.690 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[4] CRLC ? CRLC_Config_CNF = PDU: { cellId: 6 , routingInfo: [rB_Identity: 0 ]} Attach:[19] Exit Test Step ts_SS_RB0_Cfg
Attach:[20] Enter Test Step ts_SetCellCfg( 6 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 6 )
| Assignment:[14] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Assignment:[2] cellConfig := cell_FACH_NoDedicated Attach:[3] Enter Test Step ts_SaveCellInfo( 6 )
| Assignment:[14] tcv_CellInfoG := (view Assignment) Attach:[3] Exit Test Step ts_SaveCellInfo
Attach:[20] Exit Test Step ts_SetCellCfg
Attach:[23] Exit Test Step ts_SS_CreateCellFACH
Attach:[24] Enter Test Step ts_SendDefSysInfo_PLMN( 6 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 6 )
| Assignment:[14] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[2] Enter Test Step ts_UTRAN_GERAN_ParaInit( 6 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 6 )
| Assignment:[14] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Assignment:[3] tcv_SIB3 := (view Assignment) Assignment:[3] tcv_SIB4 := (view Assignment) Attach:[2] Exit Test Step ts_UTRAN_GERAN_ParaInit
Attach:[3] Enter Test Step ts_CellDependentPara( 6 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 6 )
| Assignment:[14] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Assignment:[15] cellIdentity := '0000000000000000000000000110'B Assignment:[15] cellIdentity := '0000000000000000000000000110'B Attach:[3] Exit Test Step ts_CellDependentPara
Attach:[4] Enter Test Step ts_InitializeSIB2AndSIB18( { cellId: 4 , frequenc ...
| (view Test Step parameters) Assignment:[1] tcv_SIB2 := { ura_IdentityList: [ '0000000000000100'B ] , nonCriticalExtensions: OMIT} Attach:[7] Enter Test Step ts_InitializeSIB2AndSIB18::lt_Init3PLMN( { cellId: 4 , frequenc ...
| (view Test Step parameters) Assignment:[16] tcv_SIB18 := (view Assignment) Attach:[7] Exit Test Step ts_InitializeSIB2AndSIB18::lt_Init3PLMN
Attach:[4] Exit Test Step ts_InitializeSIB2AndSIB18
Attach:[5] Enter Test Step ts_InitializeSIB11_12_SIB12_Idle( 6 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 6 )
| Assignment:[14] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[7] Enter Test Step ts_InitializeSIB11_12_SIB12_Idle::lt_3PLMN( 6 )
| Assignment:[39] tcv_SIB11 := (view Assignment) Assignment:[39] tcv_SIB12 := (view Assignment) Attach:[7] Exit Test Step ts_InitializeSIB11_12_SIB12_Idle::lt_3PLMN
Attach:[5] Exit Test Step ts_InitializeSIB11_12_SIB12_Idle
Assignment:[6] tcv_MIB := (view Assignment) Assignment:[6] tcv_SB1 := (view Assignment) Attach:[8] Enter Test Step ts_SendSIB1_LongNeighCellInfo( { cn_CommonGSM_MAP_NAS ...
| (view Test Step parameters) Assignment:[1] tcv_SIB1 := (view Assignment) 00:01:15.710 - Primitive: o_SIB_PER_Encoding Assignment:[1] seg1 := (view Assignment) 00:01:15.710 - Primitive: o_SIB_PER_Encoding Assignment:[1] seg2 := '00000000000000000100'B Attach:[4] Enter Test Step ts_Scheduling( 6 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:01:15.710 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[4] Exit Test Step ts_Scheduling
00:01:15.720 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[5] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 6 , routingInfo: [rB_Identity: -1 ]} 00:01:15.720 - Primitive: RLC_TR_DATA_REQ 00:01:15.720 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[6] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Assignment:[7] sysInfoType1 := 2 Attach:[8] Enter Test Step ts_ChangeMIB_ValueTag( )
| Assignment:[2] mib_ValueTag := 2 Assignment:[2] tcv_MIB_ValueTagChanged := GcTRUE Attach:[8] Exit Test Step ts_ChangeMIB_ValueTag
Attach:[8] Exit Test Step ts_SendSIB1_LongNeighCellInfo
Attach:[9] Enter Test Step ts_SendSIB2_LongNeighCellInfo( { ura_IdentityList: [ ...
| (view Test Step parameters) Assignment:[1] tcv_SIB2 := { ura_IdentityList: [ '0000000000000100'B ] , nonCriticalExtensions: OMIT} 00:01:15.720 - Primitive: o_SIB_PER_Encoding Assignment:[1] seg1 := '00000000000000000100'B 00:01:15.720 - Primitive: o_SIB_PER_Encoding Assignment:[1] seg2 := (view Assignment) Attach:[4] Enter Test Step ts_Scheduling( 6 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:01:15.720 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[4] Exit Test Step ts_Scheduling
00:01:15.740 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[5] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 6 , routingInfo: [rB_Identity: -1 ]} 00:01:15.740 - Primitive: RLC_TR_DATA_REQ 00:01:15.740 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[6] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Assignment:[7] sysInfoType2 := 2 Attach:[8] Enter Test Step ts_ChangeMIB_ValueTag( )
| Attach:[8] Exit Test Step ts_ChangeMIB_ValueTag
Attach:[9] Exit Test Step ts_SendSIB2_LongNeighCellInfo
Attach:[10] Enter Test Step ts_SendSIB3_LongNeighCellInfo( { sib4indicator: GcTRU ...
| (view Test Step parameters) Assignment:[1] tcv_SIB3 := (view Assignment) 00:01:15.740 - Primitive: o_SIB_PER_Encoding Assignment:[1] seg1 := (view Assignment) 00:01:15.750 - Primitive: o_SIB_PER_Encoding Assignment:[1] seg2 := '100000101000000010000001'B Attach:[4] Enter Test Step ts_Scheduling( 6 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:01:15.750 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[4] Exit Test Step ts_Scheduling
00:01:15.770 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[5] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 6 , routingInfo: [rB_Identity: -1 ]} 00:01:15.770 - Primitive: RLC_TR_DATA_REQ 00:01:15.770 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[6] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Assignment:[7] sysInfoType3 := 2 Attach:[8] Enter Test Step ts_ChangeMIB_ValueTag( )
| Attach:[8] Exit Test Step ts_ChangeMIB_ValueTag
Attach:[10] Exit Test Step ts_SendSIB3_LongNeighCellInfo
Attach:[11] Enter Test Step ts_SendSIB4_LongNeighCellInfo( { cellIdentity: '00000 ...
| (view Test Step parameters) Assignment:[1] tcv_SIB4 := (view Assignment) 00:01:15.770 - Primitive: o_SIB_PER_Encoding Assignment:[1] seg1 := (view Assignment) 00:01:15.770 - Primitive: o_SIB_PER_Encoding Assignment:[1] seg2 := '100000101000000010000001'B Attach:[4] Enter Test Step ts_Scheduling( 6 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:01:15.770 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[4] Exit Test Step ts_Scheduling
00:01:15.790 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[5] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 6 , routingInfo: [rB_Identity: -1 ]} 00:01:15.790 - Primitive: RLC_TR_DATA_REQ 00:01:15.790 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[6] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Assignment:[7] sysInfoType4 := 2 Attach:[8] Enter Test Step ts_ChangeMIB_ValueTag( )
| Attach:[8] Exit Test Step ts_ChangeMIB_ValueTag
Attach:[11] Exit Test Step ts_SendSIB4_LongNeighCellInfo
Attach:[12] Enter Test Step ts_SendSIB5_LongNeighCellInfo( { sib6indicator: GcTRU ...
| (view Test Step parameters) 00:01:15.800 - Primitive: o_SIB_PER_Encoding Assignment:[1] tcv_Segs := (view Assignment) Assignment:[38] sysInfoType5 := 2 Assignment:[38] scheduling := (view Assignment) Attach:[39] Enter Test Step ts_ChangeMIB_ValueTag( )
| Attach:[39] Exit Test Step ts_ChangeMIB_ValueTag
Attach:[40] Enter Test Step ts_Scheduling( 6 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:01:15.820 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[40] Exit Test Step ts_Scheduling
00:01:15.830 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[41] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 6 , routingInfo: [rB_Identity: -1 ]} 00:01:15.830 - Primitive: RLC_TR_DATA_REQ 00:01:15.830 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[42] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[43] Enter Test Step ts_Scheduling( 6 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:01:15.830 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[43] Exit Test Step ts_Scheduling
00:01:15.850 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[44] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 6 , routingInfo: [rB_Identity: -1 ]} 00:01:15.850 - Primitive: RLC_TR_DATA_REQ 00:01:15.850 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[45] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[46] Enter Test Step ts_Scheduling( 6 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:01:15.850 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[46] Exit Test Step ts_Scheduling
00:01:15.860 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[47] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 6 , routingInfo: [rB_Identity: -1 ]} 00:01:15.860 - Primitive: RLC_TR_DATA_REQ 00:01:15.860 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[48] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[49] Enter Test Step ts_Scheduling( 6 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:01:15.860 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[49] Exit Test Step ts_Scheduling
00:01:15.880 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[50] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 6 , routingInfo: [rB_Identity: -1 ]} 00:01:15.880 - Primitive: RLC_TR_DATA_REQ 00:01:15.880 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[52] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[12] Exit Test Step ts_SendSIB5_LongNeighCellInfo
Attach:[13] Enter Test Step ts_SendSIB6_LongNeighCellInfo( { pich_PowerOffset: -5 ...
| (view Test Step parameters) 00:01:15.880 - Primitive: o_SIB_PER_Encoding Assignment:[1] tcv_Segs := (view Assignment) Assignment:[5] sysInfoType6 := 2 Assignment:[5] scheduling := { scheduling: { segCount: OMIT, sib_Pos: [rep64: 2 ], sib_PosOffsetInfo: OMIT} } Attach:[6] Enter Test Step ts_ChangeSB1_ValueTag( )
| Assignment:[2] tcv_SB1_ValueTag := 2 Assignment:[2] sysInfoTypeSB1 := 2 Assignment:[2] tcv_SB1_ValueTagChanged := GcTRUE Attach:[3] Enter Test Step ts_ChangeMIB_ValueTag( )
| Attach:[3] Exit Test Step ts_ChangeMIB_ValueTag
Attach:[6] Exit Test Step ts_ChangeSB1_ValueTag
Attach:[7] Enter Test Step ts_Scheduling( 6 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:01:15.880 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[7] Exit Test Step ts_Scheduling
00:01:15.890 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[8] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 6 , routingInfo: [rB_Identity: -1 ]} Attach:[9] Enter Test Step ts_SendSIB6_LongNeighCellInfo::lt_CompleteSIB( systemInformationBlockType6 )
| 00:01:15.890 - Primitive: RLC_TR_DATA_REQ 00:01:15.890 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[76] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[9] Exit Test Step ts_SendSIB6_LongNeighCellInfo::lt_CompleteSIB
Attach:[10] Enter Test Step ts_Scheduling( 6 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:01:15.890 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[10] Exit Test Step ts_Scheduling
00:01:15.910 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[11] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 6 , routingInfo: [rB_Identity: -1 ]} 00:01:15.910 - Primitive: RLC_TR_DATA_REQ 00:01:15.910 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[12] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[13] Enter Test Step ts_Scheduling( 6 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:01:15.910 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[13] Exit Test Step ts_Scheduling
00:01:15.930 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[14] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 6 , routingInfo: [rB_Identity: -1 ]} 00:01:15.930 - Primitive: RLC_TR_DATA_REQ 00:01:15.930 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[15] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[16] Enter Test Step ts_Scheduling( 6 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:01:15.930 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[16] Exit Test Step ts_Scheduling
00:01:15.940 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[17] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 6 , routingInfo: [rB_Identity: -1 ]} 00:01:15.940 - Primitive: RLC_TR_DATA_REQ 00:01:15.940 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[18] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[13] Exit Test Step ts_SendSIB6_LongNeighCellInfo
Attach:[14] Enter Test Step ts_SendSIB7_LongNeighCellInfo( { modeSpecificInfo: [f ...
| (view Test Step parameters) 00:01:15.940 - Primitive: o_SIB_PER_Encoding Assignment:[1] tcv_Segs := (view Assignment) Assignment:[1] tcv_SIB7 := (view Assignment) 00:01:15.940 - Primitive: o_SIB_PER_Encoding Assignment:[1] tcv_Segs_SIB12 := (view Assignment) Attach:[4] Enter Test Step ts_Scheduling( 6 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:01:15.960 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[4] Exit Test Step ts_Scheduling
00:01:15.970 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[5] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 6 , routingInfo: [rB_Identity: -1 ]} Attach:[6] Enter Test Step ts_SendSIB7_LongNeighCellInfo::lt_CompleteSIB7OrLastSIB12_CompleteSIB7( { modeSpecificInfo: [f ...
| (view Test Step parameters) 00:01:15.970 - Primitive: RLC_TR_DATA_REQ 00:01:15.970 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[36] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[6] Exit Test Step ts_SendSIB7_LongNeighCellInfo::lt_CompleteSIB7OrLastSIB12_CompleteSIB7
Attach:[7] Enter Test Step ts_SendSIB7_LongNeighCellInfo::lt_ConcatWithSIB3( { modeSpecificInfo: [f ...
| (view Test Step parameters) 00:01:15.970 - Primitive: o_SIB_PER_Encoding Assignment:[10] seg2 := (view Assignment) Attach:[13] Enter Test Step ts_Scheduling( 6 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:01:15.970 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[13] Exit Test Step ts_Scheduling
00:01:15.990 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[14] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 6 , routingInfo: [rB_Identity: -1 ]} 00:01:15.990 - Primitive: RLC_TR_DATA_REQ 00:01:15.990 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[15] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[7] Exit Test Step ts_SendSIB7_LongNeighCellInfo::lt_ConcatWithSIB3
Attach:[8] Enter Test Step ts_SendSIB7_LongNeighCellInfo::lt_ConcatWithSIB18( { modeSpecificInfo: [f ...
| (view Test Step parameters) 00:01:15.990 - Primitive: o_SIB_PER_Encoding Assignment:[16] seg2 := (view Assignment) Attach:[19] Enter Test Step ts_Scheduling( 6 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:01:15.990 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[19] Exit Test Step ts_Scheduling
00:01:16.000 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[20] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 6 , routingInfo: [rB_Identity: -1 ]} 00:01:16.000 - Primitive: RLC_TR_DATA_REQ 00:01:16.000 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[21] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[8] Exit Test Step ts_SendSIB7_LongNeighCellInfo::lt_ConcatWithSIB18
Attach:[9] Enter Test Step ts_SendSIB7_LongNeighCellInfo::lt_ConcatWithSIB4( { modeSpecificInfo: [f ...
| (view Test Step parameters) 00:01:16.000 - Primitive: o_SIB_PER_Encoding Assignment:[22] seg2 := (view Assignment) Attach:[25] Enter Test Step ts_Scheduling( 6 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:01:16.000 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[25] Exit Test Step ts_Scheduling
00:01:16.020 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[26] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 6 , routingInfo: [rB_Identity: -1 ]} 00:01:16.020 - Primitive: RLC_TR_DATA_REQ 00:01:16.020 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[27] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[9] Exit Test Step ts_SendSIB7_LongNeighCellInfo::lt_ConcatWithSIB4
Attach:[14] Exit Test Step ts_SendSIB7_LongNeighCellInfo
Attach:[15] Enter Test Step ts_SendSIB11_LongNeighCellInfo( { sib12indicator: GcTR ...
| (view Test Step parameters) 00:01:16.040 - Primitive: o_SIB_PER_Encoding Assignment:[1] tcv_Segs := (view Assignment) Assignment:[38] sysInfoType11 := 2 Assignment:[38] scheduling := (view Assignment) Attach:[39] Enter Test Step ts_ChangeSB1_ValueTag( )
| Attach:[39] Exit Test Step ts_ChangeSB1_ValueTag
Attach:[40] Enter Test Step ts_Scheduling( 6 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:01:16.050 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[40] Exit Test Step ts_Scheduling
00:01:16.070 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[41] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 6 , routingInfo: [rB_Identity: -1 ]} 00:01:16.070 - Primitive: RLC_TR_DATA_REQ 00:01:16.070 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[42] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[43] Enter Test Step ts_Scheduling( 6 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:01:16.070 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[43] Exit Test Step ts_Scheduling
00:01:16.080 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[44] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 6 , routingInfo: [rB_Identity: -1 ]} 00:01:16.080 - Primitive: RLC_TR_DATA_REQ 00:01:16.080 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[45] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[46] Enter Test Step ts_Scheduling( 6 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:01:16.080 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[46] Exit Test Step ts_Scheduling
00:01:16.100 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[47] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 6 , routingInfo: [rB_Identity: -1 ]} 00:01:16.100 - Primitive: RLC_TR_DATA_REQ 00:01:16.100 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[48] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[49] Enter Test Step ts_Scheduling( 6 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:01:16.100 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[49] Exit Test Step ts_Scheduling
00:01:16.110 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[50] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 6 , routingInfo: [rB_Identity: -1 ]} 00:01:16.110 - Primitive: RLC_TR_DATA_REQ 00:01:16.110 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[52] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[15] Exit Test Step ts_SendSIB11_LongNeighCellInfo
Attach:[16] Enter Test Step ts_SendSIB12_LongNeighCellInfo( { fach_MeasurementOcca ...
| (view Test Step parameters) 00:01:16.110 - Primitive: o_SIB_PER_Encoding Assignment:[1] tcv_Segs_SIB12 := (view Assignment) Assignment:[38] sysInfoType12 := 2 Assignment:[38] scheduling := (view Assignment) Attach:[39] Enter Test Step ts_ChangeSB1_ValueTag( )
| Attach:[39] Exit Test Step ts_ChangeSB1_ValueTag
Attach:[40] Enter Test Step ts_Scheduling( 6 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:01:16.140 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[40] Exit Test Step ts_Scheduling
00:01:16.160 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[41] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 6 , routingInfo: [rB_Identity: -1 ]} 00:01:16.160 - Primitive: RLC_TR_DATA_REQ 00:01:16.160 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[42] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[43] Enter Test Step ts_Scheduling( 6 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:01:16.160 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[43] Exit Test Step ts_Scheduling
00:01:16.180 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[44] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 6 , routingInfo: [rB_Identity: -1 ]} 00:01:16.180 - Primitive: RLC_TR_DATA_REQ 00:01:16.180 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[45] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[46] Enter Test Step ts_Scheduling( 6 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:01:16.180 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[46] Exit Test Step ts_Scheduling
00:01:16.190 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[47] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 6 , routingInfo: [rB_Identity: -1 ]} Attach:[48] Enter Test Step ts_SendSIB12_LongNeighCellInfo::lt_CompleteSIB7( { fach_MeasurementOcca ...
| (view Test Step parameters) 00:01:16.190 - Primitive: o_SIB_PER_Encoding Assignment:[74] tcv_Segs := (view Assignment) 00:01:16.190 - Primitive: RLC_TR_DATA_REQ 00:01:16.190 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[80] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[48] Exit Test Step ts_SendSIB12_LongNeighCellInfo::lt_CompleteSIB7
Attach:[49] Enter Test Step ts_Scheduling( 6 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:01:16.190 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[49] Exit Test Step ts_Scheduling
00:01:16.210 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[50] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 6 , routingInfo: [rB_Identity: -1 ]} 00:01:16.210 - Primitive: RLC_TR_DATA_REQ 00:01:16.210 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[52] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[16] Exit Test Step ts_SendSIB12_LongNeighCellInfo
Attach:[17] Enter Test Step ts_SendSIB18_LongNeighCellInfo( { idleModePLMNIdentiti ...
| (view Test Step parameters) Assignment:[1] tcv_SIB18 := (view Assignment) 00:01:16.210 - Primitive: o_SIB_PER_Encoding Assignment:[1] seg1 := (view Assignment) 00:01:16.210 - Primitive: o_SIB_PER_Encoding Assignment:[1] seg2 := '100000101000000010000001'B Attach:[4] Enter Test Step ts_Scheduling( 6 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:01:16.210 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[4] Exit Test Step ts_Scheduling
00:01:16.220 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[5] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 6 , routingInfo: [rB_Identity: -1 ]} 00:01:16.220 - Primitive: RLC_TR_DATA_REQ 00:01:16.220 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[6] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Assignment:[7] sysInfoType18 := 2 Attach:[8] Enter Test Step ts_ChangeSB1_ValueTag( )
| Attach:[8] Exit Test Step ts_ChangeSB1_ValueTag
Attach:[17] Exit Test Step ts_SendSIB18_LongNeighCellInfo
Attach:[18] Enter Test Step ts_SendSB1_LongNeighCellInfo( { sib_ReferenceList: [ ...
| (view Test Step parameters) 00:01:16.220 - Primitive: o_SIB_PER_Encoding Assignment:[1] tcv_Segs := (view Assignment) Attach:[3] Enter Test Step ts_Scheduling( 6 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:01:16.220 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[3] Exit Test Step ts_Scheduling
00:01:16.240 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[4] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 6 , routingInfo: [rB_Identity: -1 ]} Attach:[5] Enter Test Step ts_SendSB1_LongNeighCellInfo::lt_CompleteSIB( schedulingBlock1 )
| 00:01:16.240 - Primitive: RLC_TR_DATA_REQ 00:01:16.240 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[12] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[5] Exit Test Step ts_SendSB1_LongNeighCellInfo::lt_CompleteSIB
Attach:[6] Enter Test Step ts_ChangeSB1_ValueTag( )
| Attach:[6] Exit Test Step ts_ChangeSB1_ValueTag
Assignment:[7] scheduling := { scheduling: { segCount: OMIT, sib_Pos: [rep16: 1 ], sib_PosOffsetInfo: OMIT} } Assignment:[7] tcv_SB1_ValueTagChanged := GcFALSE Attach:[18] Exit Test Step ts_SendSB1_LongNeighCellInfo
Attach:[19] Enter Test Step ts_SendMIB( { mib_ValueTag: 2 , pl ...
| (view Test Step parameters) Attach:[1] Enter Test Step ts_SetTmpCellInfo( 6 )
| Assignment:[14] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Assignment:[2] mcc := [ 0 , 0 , 4 ] Assignment:[2] mnc := [ 2 , 1 ] 00:01:16.240 - Primitive: o_SIB_PER_Encoding Assignment:[3] tcv_Segs := (view Assignment) Attach:[6] Enter Test Step ts_Scheduling( 6 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:01:16.270 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[6] Exit Test Step ts_Scheduling
00:01:16.290 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[7] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 6 , routingInfo: [rB_Identity: -1 ]} Attach:[8] Enter Test Step ts_SendMIB::lt_CompleteSIB( masterInformationBlock )
| 00:01:16.290 - Primitive: RLC_TR_DATA_REQ 00:01:16.290 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[13] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[8] Exit Test Step ts_SendMIB::lt_CompleteSIB
Assignment:[9] tcv_MIB_ValueTagChanged := GcFALSE Attach:[19] Exit Test Step ts_SendMIB
Attach:[20] Enter Test Step ts_SendPage1_ModifySI( 6 )
| Attach:[1] Enter Test Step ts_RRC_Delay( 5000 )
| StartTimer:[1] t_Dly [5000] 5000 ms Timed out Timer:t_Dly TimeOut:[2] t_Dly [5000] 5000 ms Attach:[1] Exit Test Step ts_RRC_Delay
Attach:[2] Enter Test Step ts_CMAC_Pag1_Cfg( 6 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 6 )
| Assignment:[14] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[3] Enter Test Step ts_CMAC_Pag1_Cfg::lt_CalculateDrxCycleLength( 6 )
| Assignment:[10] tcv_dRX_CycleLengthPaging := 7 Attach:[3] Exit Test Step ts_CMAC_Pag1_Cfg::lt_CalculateDrxCycleLength
00:01:21.300 - Primitive: CMAC_PAGING_Config_REQ Send event:[4] CMAC ! CMAC_PAGING_Config_REQ = PDU (view PDU) 00:01:21.320 - Primitive: CMAC_PAGING_Config_CNF begin "ca_CMAC_PagingCfgCnf" of type CMAC_PAGING_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 5 against 5 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_PagingCfgCnf" of type CMAC_PAGING_Config_CNF Receive event:[5] CMAC ? CMAC_PAGING_Config_CNF = PDU (view PDU) Attach:[2] Exit Test Step ts_CMAC_Pag1_Cfg
00:01:21.320 - Primitive: RLC_TR_DATA_REQ 00:01:21.320 - Primitive: RLC_TR_DATA_REQ: pagingType1 Send event:[3] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[4] Enter Test Step ts_SendSysInfoChangeInd_InFACHConfig( 6 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 6 )
| Assignment:[14] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[4] Exit Test Step ts_SendSysInfoChangeInd_InFACHConfig
Attach:[20] Exit Test Step ts_SendPage1_ModifySI
Attach:[21] Enter Test Step ts_SaveBackMIB_SB1( 6 )
| Assignment:[14] tcv_MIB_CellG := (view Assignment) Assignment:[14] tcv_SB1_CellG := (view Assignment) Attach:[21] Exit Test Step ts_SaveBackMIB_SB1
Attach:[24] Exit Test Step ts_SendDefSysInfo_PLMN
Attach:[25] Enter Test Step ts_UpdateRegistration( 6 )
| Attach:[1] Enter Test Step ts_RRC_ConnEst( 6 )
| Attach:[1] Enter Test Step ts_SS_PrepareCellRRC_ConnEst( 6 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 6 )
| Assignment:[14] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[9] Enter Test Step ts_SS_PrepareCellRRC_ConnEst::lt_ReconfOldFACH_Cell( 6 )
| Attach:[14] Enter Test Step ts_ReconfigFACH_ToNoDedicated( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
00:01:21.320 - Primitive: CMAC_Config_REQ Send event:[3] CMAC ! CMAC_Config_REQ = PDU (view PDU) 00:01:21.330 - Primitive: CMAC_Config_CNF begin "ca_CMAC_CfgCnf" of type CMAC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 5 against 5 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_CfgCnf" of type CMAC_Config_CNF Receive event:[4] CMAC ? CMAC_Config_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 5 ]} 00:01:21.330 - Primitive: CMAC_Config_REQ Send event:[5] CMAC ! CMAC_Config_REQ = PDU (view PDU) 00:01:21.360 - Primitive: CMAC_Config_CNF begin "ca_CMAC_CfgCnf" of type CMAC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 8 against 8 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_CfgCnf" of type CMAC_Config_CNF Receive event:[6] CMAC ? CMAC_Config_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 8 ]} Attach:[7] Enter Test Step ts_ReconfigFACH_ToNoDedicated::lt_RelBCCH_FACH( 0 )
| Attach:[11] Enter Test Step ts_CRLC_Rel( 0 )
| 00:01:21.360 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:21.380 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -3 against -3 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -3 ]} Attach:[11] Exit Test Step ts_CRLC_Rel
Attach:[7] Exit Test Step ts_ReconfigFACH_ToNoDedicated::lt_RelBCCH_FACH
Attach:[14] Exit Test Step ts_ReconfigFACH_ToNoDedicated
Assignment:[15] cellConfig := cell_FACH_NoDedicated Attach:[9] Exit Test Step ts_SS_PrepareCellRRC_ConnEst::lt_ReconfOldFACH_Cell
Attach:[10] Enter Test Step ts_SS_ReconfNoDedicatedToCellFACH( 6 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 6 )
| Assignment:[14] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
00:01:21.380 - Primitive: CMAC_Config_REQ Send event:[3] CMAC ! CMAC_Config_REQ = PDU (view PDU) 00:01:21.410 - Primitive: CMAC_Config_CNF begin "ca_CMAC_CfgCnf" of type CMAC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 5 against 5 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_CfgCnf" of type CMAC_Config_CNF Receive event:[4] CMAC ? CMAC_Config_CNF = PDU: { cellId: 6 , routingInfo: [physicalChannelIdentity: 5 ]} 00:01:21.410 - Primitive: CMAC_Config_REQ Send event:[5] CMAC ! CMAC_Config_REQ = PDU (view PDU) 00:01:21.440 - Primitive: CMAC_Config_CNF begin "ca_CMAC_CfgCnf" of type CMAC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 8 against 8 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_CfgCnf" of type CMAC_Config_CNF Receive event:[6] CMAC ? CMAC_Config_CNF = PDU: { cellId: 6 , routingInfo: [physicalChannelIdentity: 8 ]} Attach:[7] Enter Test Step ts_SS_ReconfNoDedicatedToCellFACH::lt_RB_BCCH_FACH_Cfg( 6 )
| Attach:[11] Enter Test Step ts_SS_RB_BCCH_FACH_Cfg( 6 )
| 00:01:21.440 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:21.460 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -3 against -3 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: 6 , routingInfo: [rB_Identity: -3 ]} Attach:[11] Exit Test Step ts_SS_RB_BCCH_FACH_Cfg
Attach:[7] Exit Test Step ts_SS_ReconfNoDedicatedToCellFACH::lt_RB_BCCH_FACH_Cfg
Attach:[10] Exit Test Step ts_SS_ReconfNoDedicatedToCellFACH
Attach:[11] Enter Test Step ts_SetCellCfg( 6 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 6 )
| Assignment:[14] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Assignment:[2] cellConfig := cell_FACH_NoConn Attach:[3] Enter Test Step ts_SaveCellInfo( 6 )
| Assignment:[14] tcv_CellInfoG := (view Assignment) Attach:[3] Exit Test Step ts_SaveCellInfo
Attach:[11] Exit Test Step ts_SetCellCfg
Attach:[1] Exit Test Step ts_SS_PrepareCellRRC_ConnEst
Attach:[2] Enter Test Step ts_SetTmpCellInfo( 6 )
| Assignment:[14] tcv_TmpCellInfo := (view Assignment) Attach:[2] Exit Test Step ts_SetTmpCellInfo
Attach:[3] Enter Test Step ts_RRC_ConnEst::lt_RcvConnReq( 6 )
| 00:01:39.470 - Primitive: RLC_TR_DATA_IND: rrcConnectionRequest 00:01:39.470 - Primitive: RLC_TR_DATA_IND begin "car_RRC_ConnReq" of type RLC_TR_DATA_IND (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "tM_message" of type CHOICE [UNIVERSAL 31] begin "uL_CCCH_Message" of type UL_CCCH_Message (SEQUENCE) [UNIVERSAL 16] begin "message" of type UL_CCCH_MessageType (CHOICE) [UNIVERSAL 31] begin "rrcConnectionRequest" of type RRCConnectionRequest (SEQUENCE) [UNIVERSAL 16] begin "initialUE_Identity" of type InitialUE_Identity (CHOICE) [UNIVERSAL 31] begin InitialUE_Identity (CHOICE) [UNIVERSAL 31] end InitialUE_Identity begin InitialUE_Identity (CHOICE) [UNIVERSAL 31] begin "tmsi_and_LAI" of type TMSI_and_LAI_GSM_MAP (SEQUENCE) [UNIVERSAL 16] matching { tmsi: '00010001001000100011001101000100'B , lai: { plmn_Identity: { mcc: [ 0 , 0 , 1 ] , mnc: [ 0 , 1 ] } , lac: '0000000000000001'B } } against ? end "tmsi_and_LAI" of type TMSI_and_LAI_GSM_MAP end InitialUE_Identity matching [tmsi_and_LAI: { tmsi: '00010001001000100011001101000100'B , lai: { plmn_Identity: { mcc: [ 0 , 0 , 1 ] , mnc: [ 0 , 1 ] } , lac: '0000000000000001'B } } ] against ([imsi: ?], [tmsi_and_LAI: ?], [p_TMSI_and_RAI: ?], [imei: ?]) end "initialUE_Identity" of type InitialUE_Identity begin "establishmentCause" of type EstablishmentCause (ENUMERATED) [UNIVERSAL 10] matching registration against registration end "establishmentCause" of type EstablishmentCause begin "protocolErrorIndicator" of type ProtocolErrorIndicator (ENUMERATED) [UNIVERSAL 10] matching noError against noError end "protocolErrorIndicator" of type ProtocolErrorIndicator end "rrcConnectionRequest" of type RRCConnectionRequest end "message" of type UL_CCCH_MessageType end "uL_CCCH_Message" of type UL_CCCH_Message end "tM_message" of type CHOICE end "car_RRC_ConnReq" of type RLC_TR_DATA_IND Assignment:[7] tcv_InitialUE_Id := (view Assignment) Receive event:[7] TM ? RLC_TR_DATA_IND = PDU (view PDU) Attach:[3] Exit Test Step ts_RRC_ConnEst::lt_RcvConnReq
Attach:[4] Enter Test Step ts_RRC_ConnEst::lt_Send_ConnSetUp( 6 )
| 00:01:39.470 - Primitive: RLC_UM_DATA_REQ 00:01:39.470 - Primitive: RLC_UM_DATA_REQ: rrcConnectionSetup Send event:[11] UM ! RLC_UM_DATA_REQ = PDU (view PDU) Attach:[13] Enter Test Step ts_SetCellCfg( 6 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 6 )
| Assignment:[14] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Assignment:[2] cellConfig := cell_FACH Attach:[3] Enter Test Step ts_SaveCellInfo( 6 )
| Assignment:[14] tcv_CellInfoG := (view Assignment) Attach:[3] Exit Test Step ts_SaveCellInfo
Attach:[13] Exit Test Step ts_SetCellCfg
Attach:[4] Exit Test Step ts_RRC_ConnEst::lt_Send_ConnSetUp
Attach:[5] Enter Test Step ts_RRC_ReceiveConnSetupCmpl( 6 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 6 )
| Assignment:[14] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
StartTimer:[8] t_WaitMS [13500] 13500 ms 00:01:40.040 - Primitive: RLC_AM_DATA_IND: rrcConnectionSetupComplete 00:01:40.050 - Primitive: RLC_AM_DATA_IND begin "car_RRC_ConnSetupCmpl" of type RLC_AM_DATA_IND (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "integrityResult" of type IntegrityResult (CHOICE) [UNIVERSAL 31] matching [integrityUsed: i_pass] against ? end "integrityResult" of type IntegrityResult begin "aM_message" of type CHOICE [UNIVERSAL 31] begin "uL_DCCH_Message" of type UL_DCCH_Message (SEQUENCE) [UNIVERSAL 16] begin "message" of type UL_DCCH_MessageType (CHOICE) [UNIVERSAL 31] begin "rrcConnectionSetupComplete" of type RRCConnectionSetupComplete (SEQUENCE) [UNIVERSAL 16] begin "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier (INTEGER) [UNIVERSAL 2] matching 0 against 0 end "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier begin "startList" of type STARTList (SEQUENCEOF) [UNIVERSAL 28] matching [ { cn_DomainIdentity: ps_domain, start_Value: '00000000000000000010'B } , { cn_DomainIdentity: cs_domain, start_Value: '00000000000000000010'B } ] against ? end "startList" of type STARTList begin "ue_RadioAccessCapability" of type UE_RadioAccessCapability (SEQUENCE) [UNIVERSAL 16] matching { accessStratumReleaseIndicator: r99, pdcp_Capability: { losslessSRNS_RelocationSupport: GcTRUE , supportForRfc2507: [supported: by8192]} , rlc_Capability: { totalRLC_AM_BufferSize: kb50, maximumRLC_WindowSize: mws2047, maximumAM_EntityNumber: am6} , transportChannelCapability: { dl_TransChCapability: { maxNoBitsReceived: b5120, maxConvCodeBitsReceived: b1280, turboDecodingSupport: [supported: b5120], maxSimultaneousTransChs: e8, maxSimultaneousCCTrCH_Count: 1 , maxReceivedTransportBlocks: tb16, maxNumberOfTFC: tfc96, maxNumberOfTF: tf64} , ul_TransChCapability: { maxNoBitsTransmitted: b3840, maxConvCodeBitsTransmitted: b1280, turboEncodingSupport: [supported: b3840], maxSimultaneousTransChs: e8, modeSpecificInfo: [fdd: NULL], maxTransmittedBlocks: tb8, maxNumberOfTFC: tfc32, maxNumberOfTF: tf32} } , rf_Capability: { fddRF_Capability: { ue_PowerClass: 4 , txRxFrequencySeparation: mhz190} , tddRF_Capability: OMIT} , physicalChannelCapability: { fddPhysChCapability: { downlinkPhysChCapability: { maxNoDPCH_PDSCH_Codes: 3 , maxNoPhysChBitsReceived: b9600, supportForSF_512: GcFALSE , supportOfPDSCH: GcFALSE , simultaneousSCCPCH_DPCH_Reception: [notSupported: NULL]} , uplinkPhysChCapability: { maxNoDPDCH_BitsTransmitted: b2400, supportOfPCPCH: GcFALSE } } , tddPhysChCapability: OMIT} , ue_MultiModeRAT_Capability: { multiRAT_CapabilityList: { supportOfGSM: GcFALSE , supportOfMulticarrier: GcFALSE } , multiModeCapability: fdd} , securityCapability: { cipheringAlgorithmCap: '0000000000000001'B , integrityProtectionAlgorithmCap: '0000000000000010'B } , ue_positioning_Capability: { standaloneLocMethodsSupported: GcFALSE , ue_BasedOTDOA_Supported: GcFALSE , networkAssistedGPS_Supported: noNetworkAssistedGPS, supportForUE_GPS_TimingOfCellFrames: GcFALSE , supportForIPDL: GcFALSE } , measurementCapability: { downlinkCompressedMode: { fdd_Measurements: GcTRUE , tdd_Measurements: OMIT, gsm_Measurements: { gsm900: GcTRUE , dcs1800: GcTRUE , gsm1900: GcFALSE } , multiCarrierMeasurements: GcFALSE } , uplinkCompressedMode: { fdd_Measurements: GcTRUE , tdd_Measurements: OMIT, gsm_Measurements: { gsm900: GcTRUE , dcs1800: GcTRUE , gsm1900: GcFALSE } , multiCarrierMeasurements: GcFALSE } } } against * end "ue_RadioAccessCapability" of type UE_RadioAccessCapability end "rrcConnectionSetupComplete" of type RRCConnectionSetupComplete end "message" of type UL_DCCH_MessageType end "uL_DCCH_Message" of type UL_DCCH_Message end "aM_message" of type CHOICE end "car_RRC_ConnSetupCmpl" of type RLC_AM_DATA_IND Assignment:TSP2: [10] tcv_StartList := (view Assignment) CancelTimer:TSP2: [10] t_WaitMS [13500] 13500 ms Receive event:TSP2: [10] AM ? RLC_AM_DATA_IND = PDU (view PDU) Preliminary verdict:TSP2: [10] (PASS) Attach:[11] Enter Test Step ts_RRC_ReceiveConnSetupCmpl::lt_GetHFN( 6 )
| Assignment:[13] tcv_Count := 2 Attach:[17] Enter Test Step ts_RRC_ReceiveConnSetupCmpl::lt_FirstValue( 6 )
| Assignment:[23] start_PS := '00000000000000000010'B Attach:[17] Exit Test Step ts_RRC_ReceiveConnSetupCmpl::lt_FirstValue
Attach:[18] Enter Test Step ts_RRC_ReceiveConnSetupCmpl::lt_SecondValue( 6 )
| Assignment:[26] start_CS := '00000000000000000010'B Attach:[18] Exit Test Step ts_RRC_ReceiveConnSetupCmpl::lt_SecondValue
Attach:[11] Exit Test Step ts_RRC_ReceiveConnSetupCmpl::lt_GetHFN
Attach:[5] Exit Test Step ts_RRC_ReceiveConnSetupCmpl
Attach:[1] Exit Test Step ts_RRC_ConnEst
Attach:[2] Enter Test Step ts_NAS_UpdateRegistration( 6 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 6 )
| Assignment:[14] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[3] Enter Test Step ts_NAS_UpdateRegistration::lt_CS_PS( 6 )
| Attach:[13] Enter Test Step ts_NAS_UpdateRegistration::lt_GMM_Registration( 6 )
| Attach:[13] Exit Test Step ts_NAS_UpdateRegistration::lt_GMM_Registration
Attach:[13] Enter Test Step ts_NAS_UpdateRegistration::lt_GMM_Registration( 6 )
| Attach:[13] Exit Test Step ts_NAS_UpdateRegistration::lt_GMM_Registration
Attach:[13] Enter Test Step ts_NAS_UpdateRegistration::lt_GMM_Registration( 6 )
| Attach:[13] Exit Test Step ts_NAS_UpdateRegistration::lt_GMM_Registration
Attach:[13] Enter Test Step ts_NAS_UpdateRegistration::lt_GMM_Registration( 6 )
| Attach:[13] Exit Test Step ts_NAS_UpdateRegistration::lt_GMM_Registration
Attach:[13] Enter Test Step ts_NAS_UpdateRegistration::lt_GMM_Registration( 6 )
| Attach:[13] Exit Test Step ts_NAS_UpdateRegistration::lt_GMM_Registration
Attach:[13] Enter Test Step ts_NAS_UpdateRegistration::lt_GMM_Registration( 6 )
| Attach:[13] Exit Test Step ts_NAS_UpdateRegistration::lt_GMM_Registration
Attach:[13] Enter Test Step ts_NAS_UpdateRegistration::lt_GMM_Registration( 6 )
| Attach:[13] Exit Test Step ts_NAS_UpdateRegistration::lt_GMM_Registration
Attach:[13] Enter Test Step ts_NAS_UpdateRegistration::lt_GMM_Registration( 6 )
| Attach:[13] Exit Test Step ts_NAS_UpdateRegistration::lt_GMM_Registration
Attach:[13] Enter Test Step ts_NAS_UpdateRegistration::lt_GMM_Registration( 6 )
| Attach:[13] Exit Test Step ts_NAS_UpdateRegistration::lt_GMM_Registration
Attach:[13] Enter Test Step ts_NAS_UpdateRegistration::lt_GMM_Registration( 6 )
| Attach:[13] Exit Test Step ts_NAS_UpdateRegistration::lt_GMM_Registration
Attach:[13] Enter Test Step ts_NAS_UpdateRegistration::lt_GMM_Registration( 6 )
| Attach:[13] Exit Test Step ts_NAS_UpdateRegistration::lt_GMM_Registration
Attach:[13] Enter Test Step ts_NAS_UpdateRegistration::lt_GMM_Registration( 6 )
| Attach:[13] Exit Test Step ts_NAS_UpdateRegistration::lt_GMM_Registration
00:01:40.330 - Primitive: RLC_AM_DATA_IND: initialDirectTransfer 00:01:40.330 - Primitive: RRC_DATA_IND: gmm:routingAreaUpdateRequest Attach:[13] Enter Test Step ts_NAS_UpdateRegistration::lt_GMM_Registration( 6 )
| begin "car_PS_InitDirectTransfer" of type RRC_DataInd (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "rB_Id" of type SS_RB_Identity (INTEGER) [UNIVERSAL 2] matching 3 against 3 end "rB_Id" of type SS_RB_Identity begin "cN_Domain" of type SS_CN_DomainIdentity (INTEGER) [UNIVERSAL 2] matching 1 against 1 end "cN_Domain" of type SS_CN_DomainIdentity begin "start" of type START_Value (BITSTRING) [UNIVERSAL 3] matching '00000000000000000010'B against ? end "start" of type START_Value begin "msg" of type ROUTINGAREAUPDATEREQUEST (SEQUENCE) [UNIVERSAL 16] begin "skipIndicator" of type SkipIndicator (BITSTRING) [UNIVERSAL 3] matching '0000'B against '0000'B end "skipIndicator" of type SkipIndicator begin "gMMProtocolDiscriminator" of type ProtocolDiscriminator (BITSTRING) [UNIVERSAL 3] matching '1000'B against '1000'B end "gMMProtocolDiscriminator" of type ProtocolDiscriminator begin "msgType" of type MsgType (BITSTRING) [UNIVERSAL 3] matching '00001000'B against '00001000'B end "msgType" of type MsgType begin "gprsCiphKeySeqNo" of type CiphKeySeqNum (SEQUENCE) [UNIVERSAL 16] begin "spare1" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against '0'B end "spare1" of type B1 begin "keySeq" of type KeySeq (BITSTRING) [UNIVERSAL 3] matching '000'B against ? end "keySeq" of type KeySeq end "gprsCiphKeySeqNo" of type CiphKeySeqNum begin "updateType" of type UpdateType_v (SEQUENCE) [UNIVERSAL 16] begin "for" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against ? end "for" of type B1 begin "value" of type B3 (BITSTRING) [UNIVERSAL 3] matching '001'B against ? end "value" of type B3 end "updateType" of type UpdateType_v begin "oldRAI" of type RAI_v (SEQUENCE) [UNIVERSAL 16] begin "plmn" of type OCTETSTRING [UNIVERSAL 4] matching '00F110'O against ? end "plmn" of type OCTETSTRING begin "lac" of type OCTETSTRING [UNIVERSAL 4] matching '0001'O against ? end "lac" of type OCTETSTRING begin "rac" of type OCTETSTRING [UNIVERSAL 4] matching '01'O against ? end "rac" of type OCTETSTRING end "oldRAI" of type RAI_v begin "msRadioAccessCap" of type MSRadioAccessCap_lv (SEQUENCE) [UNIVERSAL 16] matching { iel: '0A'O , value: '14F382334C03263CA060'O } against ? end "msRadioAccessCap" of type MSRadioAccessCap_lv begin "oldPTMSI_Signature" of type PTMSI_Signature (SEQUENCE) [UNIVERSAL 16] begin "iei" of type IEI8 (BITSTRING) [UNIVERSAL 3] matching '00011001'B against '00011001'B end "iei" of type IEI8 begin "value" of type OCTETSTRING [UNIVERSAL 4] matching 'AB1234'O against ? end "value" of type OCTETSTRING end "oldPTMSI_Signature" of type PTMSI_Signature begin "readyTimer" of type GPRS_Timer (SEQUENCE) [UNIVERSAL 16] begin "iei" of type IEI8 (BITSTRING) [UNIVERSAL 3] matching '00010111'B against '00010111'B end "iei" of type IEI8 begin "unit" of type B3 (BITSTRING) [UNIVERSAL 3] matching '000'B against ? end "unit" of type B3 begin "value" of type B5 (BITSTRING) [UNIVERSAL 3] matching '10110'B against ? end "value" of type B5 end "readyTimer" of type GPRS_Timer begin "drxParameter" of type DRXparamter_tv (SEQUENCE) [UNIVERSAL 16] begin "iei" of type IEI8 (BITSTRING) [UNIVERSAL 3] matching '00100111'B against '00100111'B end "iei" of type IEI8 begin "splitPGcycleCode" of type B8 (BITSTRING) [UNIVERSAL 3] matching '00000111'B against ? end "splitPGcycleCode" of type B8 begin "cnDRXcoef" of type B4 (BITSTRING) [UNIVERSAL 3] matching '0000'B against ? end "cnDRXcoef" of type B4 begin "splitOnCCCH" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against ? end "splitOnCCCH" of type B1 begin "nonDRXtimer" of type B3 (BITSTRING) [UNIVERSAL 3] matching '010'B against ? end "nonDRXtimer" of type B3 end "drxParameter" of type DRXparamter_tv begin "ptmsi" of type GMM_MS_IdentityPTMSI (SEQUENCE) [UNIVERSAL 16] begin "iei" of type IEI8 (BITSTRING) [UNIVERSAL 3] matching '00011000'B against '00011000'B end "iei" of type IEI8 begin "iel" of type Length (OCTETSTRING) [UNIVERSAL 4] matching '05'O against '05'O end "iel" of type Length begin "iDigit1" of type B4 (BITSTRING) [UNIVERSAL 3] matching '1111'B against '1111'B end "iDigit1" of type B4 begin "oddEvenInd" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against '0'B end "oddEvenInd" of type B1 begin "typeOfId" of type B3 (BITSTRING) [UNIVERSAL 3] matching '100'B against '100'B end "typeOfId" of type B3 begin "otherDigits" of type OCTETSTRING [UNIVERSAL 4] matching '12345678'O against ? end "otherDigits" of type OCTETSTRING end "ptmsi" of type GMM_MS_IdentityPTMSI begin "msnetworkcap" of type MS_NetworkCap_tlv (SEQUENCE) [UNIVERSAL 16] begin "iei" of type IEI8 (BITSTRING) [UNIVERSAL 3] matching '00110001'B against '00110001'B end "iei" of type IEI8 begin "iel" of type Length (OCTETSTRING) [UNIVERSAL 4] matching '02'O against ? end "iel" of type Length begin "value" of type OCTETSTRING [UNIVERSAL 4] matching 'E540'O against ? end "value" of type OCTETSTRING end "msnetworkcap" of type MS_NetworkCap_tlv begin "pDP_ContextStatus" of type PDP_ContextStatus (SEQUENCE) [UNIVERSAL 16] begin "iei" of type IEI8 (BITSTRING) [UNIVERSAL 3] matching '00110010'B against '00110010'B end "iei" of type IEI8 begin "iel" of type Length (OCTETSTRING) [UNIVERSAL 4] matching '02'O against ? end "iel" of type Length begin "nSAPI" of type BITSTRING [UNIVERSAL 3] matching '0000000000000000'B against ? end "nSAPI" of type BITSTRING end "pDP_ContextStatus" of type PDP_ContextStatus end "msg" of type ROUTINGAREAUPDATEREQUEST end "car_PS_InitDirectTransfer" of type RRC_DataInd Assignment:[33] tcv_TmpRAU_ReqPDU (view PDU) Assignment:[33] tcv_Start := '00000000000000000010'B Receive event:[33] Dc ? RRC_DataInd = PDU (view PDU) Attach:[34] Enter Test Step ts_NAS_UpdateRegistration::lt_GMM_RegistrationContinue( 6 )
| Attach:[35] Enter Test Step ts_SS_SecurityDownloadStart( ps_domain )
| Assignment:[4] start_PS := '00000000000000000010'B Attach:[35] Exit Test Step ts_SS_SecurityDownloadStart
Attach:[36] Enter Test Step ts_GMM_Authentication( 6 )
| Attach:[1] Enter Test Step ts_GMM_AuthenticationInit( )
| Attach:[1] Enter Test Step ts_GMM_AuthenticationInit::lt_IncrementCiphKeySeqNum( )
| Assignment:[6] tcv_PS_KeySeq := '001'B Attach:[1] Exit Test Step ts_GMM_AuthenticationInit::lt_IncrementCiphKeySeqNum
Attach:[2] Enter Test Step ts_GMM_AuthenticationInit::lt_AuthCalcAUTN( )
| Assignment:[19] tcv_AuthXDOUT := (view Assignment) Assignment:[20] tcv_AuthCDOUT := '0000000000000000000000000000000000000000000000000000000000000000'B Assignment:[21] tcv_AuthXDOUT_Half := '0101010101000100011101110110011000010001000000000011001100100010'B Assignment:[22] tcv_AuthAK := '011001100001000100000000001100110010001011011101'B Assignment:[23] tcv_AuthAUTN_1 := '011001100001000100000000001100110010001011011101'B Assignment:[24] tcv_AuthMAC := '0101010101000100011101110110011000010001000000000011001100100010'B Assignment:[25] tcv_AuthAUTN_2 := (view Assignment) Assignment:[26] tcv_AuthAUTN := (view Assignment) Attach:[2] Exit Test Step ts_GMM_AuthenticationInit::lt_AuthCalcAUTN
Attach:[3] Enter Test Step ts_GMM_AuthenticationInit::lt_AuthCalcUMTS_Others( )
| Assignment:[27] tcv_PS_AuthIK := (view Assignment) Assignment:[28] tcv_PS_AuthCK := (view Assignment) Assignment:[29] tcv_AuthXRES := (view Assignment) Attach:[3] Exit Test Step ts_GMM_AuthenticationInit::lt_AuthCalcUMTS_Others
Attach:[4] Enter Test Step ts_GMM_AuthenticationInit::lt_AuthCalcKcGSM( )
| Assignment:[30] tcv_AuthCK_1 := '0100010001110111011001100001000100000000001100110010001011011101'B Assignment:[31] tcv_AuthCK_2 := '1100110011111111111011101001100110001000101110111010101001010101'B Assignment:[32] tcv_AuthIK_1 := '0111011101100110000100010000000000110011001000101101110111001100'B Assignment:[33] tcv_AuthIK_2 := '1111111111101110100110011000100010111011101010100101010101000100'B Assignment:[34] tcv_AuthCK_XOR := '1000100010001000100010001000100010001000100010001000100010001000'B Assignment:[35] tcv_AuthIK_XOR := '1000100010001000100010001000100010001000100010001000100010001000'B Assignment:[36] tcv_AuthKcGSM := '0000000000000000000000000000000000000000000000000000000000000000'B Attach:[4] Exit Test Step ts_GMM_AuthenticationInit::lt_AuthCalcKcGSM
Attach:[1] Exit Test Step ts_GMM_AuthenticationInit
00:01:40.360 - Primitive: RRC_DATA_REQ: gmm:authenticationAndCipheringRequest 00:01:40.360 - Primitive: RLC_AM_DATA_REQ:downlinkDirectTransfer Send event:[2] Dc ! RRC_DataReq = PDU (view PDU) 00:01:40.900 - Primitive: RLC_AM_DATA_IND: uplinkDirectTransfer 00:01:40.900 - Primitive: RRC_DATA_IND: gmm:authenticationAndCipheringResponse begin "car_PS_UplinkDirectTransfer" of type RRC_DataInd (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "rB_Id" of type SS_RB_Identity (INTEGER) [UNIVERSAL 2] matching 3 against 3 end "rB_Id" of type SS_RB_Identity begin "cN_Domain" of type SS_CN_DomainIdentity (INTEGER) [UNIVERSAL 2] matching 1 against 1 end "cN_Domain" of type SS_CN_DomainIdentity begin "msg" of type AUTHENTICATIONANDCIPHERINGRESPONSE (SEQUENCE) [UNIVERSAL 16] begin "skipIndicator" of type SkipIndicator (BITSTRING) [UNIVERSAL 3] matching '0000'B against '0000'B end "skipIndicator" of type SkipIndicator begin "gMMProtocolDiscriminator" of type ProtocolDiscriminator (BITSTRING) [UNIVERSAL 3] matching '1000'B against '1000'B end "gMMProtocolDiscriminator" of type ProtocolDiscriminator begin "msgType" of type MsgType (BITSTRING) [UNIVERSAL 3] matching '00010011'B against '00010011'B end "msgType" of type MsgType begin "spare4" of type B4 (BITSTRING) [UNIVERSAL 3] matching '0000'B against '0000'B end "spare4" of type B4 begin "acRefNo" of type AC_ReferenceNumber (SEQUENCE) [UNIVERSAL 16] matching { value: '0011'B } against ? end "acRefNo" of type AC_ReferenceNumber begin "authRsp" of type AuthRsp_tv (SEQUENCE) [UNIVERSAL 16] begin "iei" of type IEI8 (BITSTRING) [UNIVERSAL 3] matching '00100010'B against '00100010'B end "iei" of type IEI8 begin "value" of type BITSTRING [UNIVERSAL 3] matching '01010101010001000111011101100110'B against ? end "value" of type BITSTRING end "authRsp" of type AuthRsp_tv begin "authRspExt" of type AuthRspExt (SEQUENCE) [UNIVERSAL 16] begin "iei" of type IEI8 (BITSTRING) [UNIVERSAL 3] matching '00101001'B against '00101001'B end "iei" of type IEI8 begin "iel" of type Length (OCTETSTRING) [UNIVERSAL 4] matching '0C'O against ? end "iel" of type Length begin "rES" of type BITSTRING [UNIVERSAL 3] matching '000100010000000000110011001000101101110111001100111111111110111010011001100010001011101110101010'B against ? end "rES" of type BITSTRING end "authRspExt" of type AuthRspExt end "msg" of type AUTHENTICATIONANDCIPHERINGRESPONSE end "car_PS_UplinkDirectTransfer" of type RRC_DataInd Assignment:[3] tcv_TmpAuthAndCiphRspPDU (view PDU) Assignment:[3] tcv_AuthRsp := '01010101010001000111011101100110'B Assignment:[3] tcv_AuthRspExt := (view Assignment) Receive event:[3] Dc ? RRC_DataInd = PDU (view PDU) Assignment:[4] tcv_Res := GcTRUE Preliminary verdict:TSP1: [6] (PASS) Attach:[36] Exit Test Step ts_GMM_Authentication
Attach:[37] Enter Test Step ts_RRC_Security( 6 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 6 )
| Assignment:[14] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[2] Enter Test Step ts_RRC_Security::lt_RRC_InitVariables( 6 )
| Attach:[53] Enter Test Step ts_RRC_Security::lt_InitCipherMode( 6 )
| Assignment:[82] cs_cipheringStarted := GcFALSE Assignment:[82] ps_cipheringStarted := GcFALSE Assignment:[86] cipheringAlgorithmCapability := '0000000000000001'B Attach:[53] Exit Test Step ts_RRC_Security::lt_InitCipherMode
Attach:[54] Enter Test Step ts_RRC_Security::lt_InitIntegrity( 6 )
| Assignment:[87] recentSecureDomain := ps_domain Assignment:[92] dL_Integrity := (view Assignment) Assignment:[92] integrityStarted := GcTRUE Assignment:[92] dl_IntegrityCheckInfo := (view Assignment) Assignment:[92] tcv_Int_ModifyFlag := GcFALSE Attach:[54] Exit Test Step ts_RRC_Security::lt_InitIntegrity
Attach:[55] Enter Test Step ts_InitSystemSpecificCap( )
| Assignment:[11] tcv_UE_SystemSpecificCap := 0 Attach:[55] Exit Test Step ts_InitSystemSpecificCap
Attach:[56] Enter Test Step ts_SaveCellInfo( 6 )
| Assignment:[14] tcv_CellInfoG := (view Assignment) Attach:[56] Exit Test Step ts_SaveCellInfo
Assignment:[58] tcv_HFN := '00000000000000000000'B Assignment:[62] start_PS := '00000000000000000000'B Attach:[2] Exit Test Step ts_RRC_Security::lt_RRC_InitVariables
Attach:[3] Enter Test Step ts_SS_DownloadSecurityKey( 6 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 6 )
| Assignment:[14] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[13] Enter Test Step ts_SS_DownloadSecurityKey::lt_DownloadKeyCRLC( '00000000000000000000'B )
| 00:01:40.910 - Primitive: CRLC_SecurityMode_Config_REQ 00:01:40.910 - Primitive: CRLC_SecurityMode_Config_REQ Send event:[21] CRLC ! CRLC_SecurityMode_Config_REQ = PDU (view PDU) 00:01:40.930 - Primitive: CRLC_SecurityMode_Config_CNF begin "ca_CRLC_SecurityModeCfgCnf" of type CRLC_SecurityMode_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER end "ca_CRLC_SecurityModeCfgCnf" of type CRLC_SecurityMode_Config_CNF Receive event:[22] CRLC ? CRLC_SecurityMode_Config_CNF = PDU: { cellId: -1 } Attach:[13] Exit Test Step ts_SS_DownloadSecurityKey::lt_DownloadKeyCRLC
Attach:[3] Exit Test Step ts_SS_DownloadSecurityKey
Attach:[4] Enter Test Step ts_RRC_Security::lt_ActivateSecurity_DL_SS( 6 )
| Attach:[14] Enter Test Step ts_RRC_Security::lt_InitialiseRRC_MSN( 6 )
| Attach:[25] Enter Test Step ts_SetDL_RRC_MessageSN( 6 )
| 00:01:40.930 - Primitive: CRLC_SetRRC_MessageSN_REQ Send event:[1] CRLC ! CRLC_SetRRC_MessageSN_REQ = PDU (view PDU) 00:01:40.940 - Primitive: CRLC_SetRRC_MessageSN_CNF begin "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF Receive event:[2] CRLC ? CRLC_SetRRC_MessageSN_CNF = PDU: { cellId: 6 , routingInfo: [rB_Identity: 0 ]} 00:01:40.940 - Primitive: CRLC_SetRRC_MessageSN_REQ Send event:[3] CRLC ! CRLC_SetRRC_MessageSN_REQ = PDU (view PDU) 00:01:40.960 - Primitive: CRLC_SetRRC_MessageSN_CNF begin "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF Receive event:[4] CRLC ? CRLC_SetRRC_MessageSN_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 1 ]} 00:01:40.960 - Primitive: CRLC_SetRRC_MessageSN_REQ Send event:[5] CRLC ! CRLC_SetRRC_MessageSN_REQ = PDU (view PDU) 00:01:40.970 - Primitive: CRLC_SetRRC_MessageSN_CNF begin "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF Receive event:[6] CRLC ? CRLC_SetRRC_MessageSN_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 2 ]} 00:01:40.970 - Primitive: CRLC_SetRRC_MessageSN_REQ Send event:[7] CRLC ! CRLC_SetRRC_MessageSN_REQ = PDU (view PDU) 00:01:40.990 - Primitive: CRLC_SetRRC_MessageSN_CNF begin "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF Receive event:[8] CRLC ? CRLC_SetRRC_MessageSN_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 3 ]} 00:01:40.990 - Primitive: CRLC_SetRRC_MessageSN_REQ Send event:[9] CRLC ! CRLC_SetRRC_MessageSN_REQ = PDU (view PDU) 00:01:41.000 - Primitive: CRLC_SetRRC_MessageSN_CNF begin "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF Receive event:[10] CRLC ? CRLC_SetRRC_MessageSN_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 4 ]} Attach:[25] Exit Test Step ts_SetDL_RRC_MessageSN
Attach:[14] Exit Test Step ts_RRC_Security::lt_InitialiseRRC_MSN
Attach:[15] Enter Test Step ts_CRLC_DL_Integrity( { integrityProtectionM ...
| (view Test Step parameters) 00:01:41.000 - Primitive: CRLC_Integrity_Activate_REQ 00:01:41.000 - Primitive: CRLC_Integrity_Activate_REQ Send event:[1] CRLC ! CRLC_Integrity_Activate_REQ = PDU (view PDU) 00:01:41.020 - Primitive: CRLC_Integrity_Activate_CNF begin "ca_CRLC_IntegrityActivateCnf" of type CRLC_Integrity_Activate_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER end "ca_CRLC_IntegrityActivateCnf" of type CRLC_Integrity_Activate_CNF Receive event:[2] CRLC ? CRLC_Integrity_Activate_CNF = PDU: { cellId: -1 } Attach:[15] Exit Test Step ts_CRLC_DL_Integrity
Attach:[4] Exit Test Step ts_RRC_Security::lt_ActivateSecurity_DL_SS
Attach:[5] Enter Test Step ts_RRC_Security::lt_RB2_UL_IntegrityActivate( 6 )
| Attach:[13] Enter Test Step ts_RB2_UL_IntegrityActivate( 0 )
| 00:01:41.020 - Primitive: CRLC_Integrity_Activate_REQ Send event:[1] CRLC ! CRLC_Integrity_Activate_REQ = PDU (view PDU) 00:01:41.040 - Primitive: CRLC_Integrity_Activate_CNF begin "ca_CRLC_IntegrityActivateCnf" of type CRLC_Integrity_Activate_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER end "ca_CRLC_IntegrityActivateCnf" of type CRLC_Integrity_Activate_CNF Receive event:[2] CRLC ? CRLC_Integrity_Activate_CNF = PDU: { cellId: -1 } Attach:[13] Exit Test Step ts_RB2_UL_IntegrityActivate
Attach:[5] Exit Test Step ts_RRC_Security::lt_RB2_UL_IntegrityActivate
Attach:[6] Enter Test Step ts_RRC_Security::lt_StartSecurity_UE( 6 )
| Attach:[27] Enter Test Step ts_RRC_Security::lt_SendSecurityModeCommand( 6 )
| 00:01:41.040 - Primitive: RLC_AM_DATA_REQ 00:01:41.040 - Primitive: RLC_AM_DATA_REQ: securityModeCommand Send event:[52] AM ! RLC_AM_DATA_REQ = PDU (view PDU) Attach:[27] Exit Test Step ts_RRC_Security::lt_SendSecurityModeCommand
00:01:41.430 - Primitive: RLC_AM_DATA_IND: securityModeComplete 00:01:41.430 - Primitive: RLC_AM_DATA_IND begin "car_RRC_SecModeCmpl" of type RLC_AM_DATA_IND (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "integrityResult" of type IntegrityResult (CHOICE) [UNIVERSAL 31] matching [integrityUsed: i_pass] against * end "integrityResult" of type IntegrityResult begin "aM_message" of type CHOICE [UNIVERSAL 31] begin "uL_DCCH_Message" of type UL_DCCH_Message (SEQUENCE) [UNIVERSAL 16] begin "integrityCheckInfo" of type IntegrityCheckInfo (SEQUENCE) [UNIVERSAL 16] matching { messageAuthenticationCode: '10001011001000110111110011100010'B , rrc_MessageSequenceNumber: 1 } against * end "integrityCheckInfo" of type IntegrityCheckInfo begin "message" of type UL_DCCH_MessageType (CHOICE) [UNIVERSAL 31] begin "securityModeComplete" of type SecurityModeComplete (SEQUENCE) [UNIVERSAL 16] begin "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier (INTEGER) [UNIVERSAL 2] matching 0 against 0 end "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier begin "ul_IntegProtActivationInfo" of type IntegrityProtActivationInfo (SEQUENCE) [UNIVERSAL 16] matching { rrc_MessageSequenceNumberList: [ 0 , 0 , 0 , 0 , 0 ] } against * end "ul_IntegProtActivationInfo" of type IntegrityProtActivationInfo end "securityModeComplete" of type SecurityModeComplete end "message" of type UL_DCCH_MessageType end "uL_DCCH_Message" of type UL_DCCH_Message end "aM_message" of type CHOICE end "car_RRC_SecModeCmpl" of type RLC_AM_DATA_IND Assignment:TSP2: [34] uL_Integrity := { rrc_MessageSequenceNumberList: [ 0 , 0 , 0 , 0 , 0 ] } Receive event:TSP2: [34] AM ? RLC_AM_DATA_IND = PDU (view PDU) Preliminary verdict:TSP2: [34] (PASS) Attach:[35] Enter Test Step ts_CRLC_UL_Integrity( { rrc_MessageSequenceNumberList: [ 0 , 0 , 0 , 0 , 0 ] } )
| 00:01:41.430 - Primitive: CRLC_Integrity_Activate_REQ Send event:[1] CRLC ! CRLC_Integrity_Activate_REQ = PDU (view PDU) 00:01:41.440 - Primitive: CRLC_Integrity_Activate_CNF begin "ca_CRLC_IntegrityActivateCnf" of type CRLC_Integrity_Activate_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER end "ca_CRLC_IntegrityActivateCnf" of type CRLC_Integrity_Activate_CNF Receive event:[2] CRLC ? CRLC_Integrity_Activate_CNF = PDU: { cellId: -1 } Attach:[35] Exit Test Step ts_CRLC_UL_Integrity
Attach:[6] Exit Test Step ts_RRC_Security::lt_StartSecurity_UE
Attach:[37] Exit Test Step ts_RRC_Security
Assignment:[38] tcv_AssignedPTMSI := '12345678'O Assignment:[38] tcv_Assigned_PTMSI_Sig := 'AB1234'O 00:01:41.440 - Primitive: RRC_DATA_REQ: gmm:routingAreaUpdateAccept 00:01:41.440 - Primitive: RLC_AM_DATA_REQ:downlinkDirectTransfer Send event:[39] Dc ! RRC_DataReq = PDU (view PDU) 00:01:41.790 - Primitive: RLC_AM_DATA_IND: uplinkDirectTransfer 00:01:41.790 - Primitive: RRC_DATA_IND: gmm:routingAreaUpdateComplete begin "car_PS_UplinkDirectTransfer" of type RRC_DataInd (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "rB_Id" of type SS_RB_Identity (INTEGER) [UNIVERSAL 2] matching 3 against 3 end "rB_Id" of type SS_RB_Identity begin "cN_Domain" of type SS_CN_DomainIdentity (INTEGER) [UNIVERSAL 2] matching 1 against 1 end "cN_Domain" of type SS_CN_DomainIdentity begin "msg" of type ROUTING_AREA_UPDATE_COMPLETE (SEQUENCE) [UNIVERSAL 16] begin "skipIndicator" of type SkipIndicator (BITSTRING) [UNIVERSAL 3] matching '0000'B against '0000'B end "skipIndicator" of type SkipIndicator begin "gMMProtocolDiscriminator" of type ProtocolDiscriminator (BITSTRING) [UNIVERSAL 3] matching '1000'B against '1000'B end "gMMProtocolDiscriminator" of type ProtocolDiscriminator begin "msgType" of type MsgType (BITSTRING) [UNIVERSAL 3] matching '00001010'B against '00001010'B end "msgType" of type MsgType end "msg" of type ROUTING_AREA_UPDATE_COMPLETE end "car_PS_UplinkDirectTransfer" of type RRC_DataInd Receive event:[40] Dc ? RRC_DataInd = PDU (view PDU) Attach:[34] Exit Test Step ts_NAS_UpdateRegistration::lt_GMM_RegistrationContinue
Attach:[13] Exit Test Step ts_NAS_UpdateRegistration::lt_GMM_Registration
Attach:[3] Exit Test Step ts_NAS_UpdateRegistration::lt_CS_PS
Attach:[4] Enter Test Step ts_NAS_UpdateRegistration::lt_RRC_ConnRel( 6 )
| Attach:[42] Enter Test Step ts_RRC_ConnRel( 6 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 6 )
| Assignment:[14] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[2] Enter Test Step ts_RRC_Delay( 1000 )
| StartTimer:[1] t_Dly [5000] 1000 ms Timed out Timer:t_Dly TimeOut:[2] t_Dly [5000] 1000 ms Attach:[2] Exit Test Step ts_RRC_Delay
Attach:[3] Enter Test Step ts_RRC_ConnRel::lt_Send_RRC_ConnectionRelease( 6 )
| 00:01:42.820 - Primitive: RLC_UM_DATA_REQ 00:01:42.820 - Primitive: RLC_UM_DATA_REQ: rrcConnectionRelease Send event:[44] UM ! RLC_UM_DATA_REQ = PDU (view PDU) 00:01:43.140 - Primitive: RLC_AM_DATA_IND: rrcConnectionReleaseComplete 00:01:43.140 - Primitive: RLC_AM_DATA_IND begin "car_RRC_ConnRelCmpl" of type RLC_AM_DATA_IND (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "integrityResult" of type IntegrityResult (CHOICE) [UNIVERSAL 31] matching [integrityUsed: i_pass] against * end "integrityResult" of type IntegrityResult begin "aM_message" of type CHOICE [UNIVERSAL 31] begin "uL_DCCH_Message" of type UL_DCCH_Message (SEQUENCE) [UNIVERSAL 16] begin "integrityCheckInfo" of type IntegrityCheckInfo (SEQUENCE) [UNIVERSAL 16] matching { messageAuthenticationCode: '00011100101000000111010101000111'B , rrc_MessageSequenceNumber: 2 } against * end "integrityCheckInfo" of type IntegrityCheckInfo begin "message" of type UL_DCCH_MessageType (CHOICE) [UNIVERSAL 31] begin "rrcConnectionReleaseComplete" of type RRCConnectionReleaseComplete (SEQUENCE) [UNIVERSAL 16] begin "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier (INTEGER) [UNIVERSAL 2] matching 0 against 0 end "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier end "rrcConnectionReleaseComplete" of type RRCConnectionReleaseComplete end "message" of type UL_DCCH_MessageType end "uL_DCCH_Message" of type UL_DCCH_Message end "aM_message" of type CHOICE end "car_RRC_ConnRelCmpl" of type RLC_AM_DATA_IND Receive event:TSP2: [45] AM ? RLC_AM_DATA_IND = PDU (view PDU) Preliminary verdict:TSP2: [45] (PASS) Attach:[46] Enter Test Step ts_RRC_Delay( 1000 )
| StartTimer:[1] t_Dly [5000] 1000 ms Timed out Timer:t_Dly TimeOut:[2] t_Dly [5000] 1000 ms Attach:[46] Exit Test Step ts_RRC_Delay
Attach:[3] Exit Test Step ts_RRC_ConnRel::lt_Send_RRC_ConnectionRelease
Attach:[4] Enter Test Step ts_RRC_ConnRel::lt_RestartCRLC_ForNextConnection( 6 )
| Attach:[10] Enter Test Step ts_CRLC_RelReconfSRB( 6 )
| Attach:[1] Enter Test Step ts_CRLC_Rel( -1 )
| 00:01:44.160 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:44.180 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 1 ]} Attach:[1] Exit Test Step ts_CRLC_Rel
Attach:[2] Enter Test Step ts_CRLC_Rel( -1 )
| 00:01:44.180 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:44.190 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 2 ]} Attach:[2] Exit Test Step ts_CRLC_Rel
Attach:[3] Enter Test Step ts_CRLC_Rel( -1 )
| 00:01:44.190 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:44.210 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 3 ]} Attach:[3] Exit Test Step ts_CRLC_Rel
Attach:[4] Enter Test Step ts_CRLC_Rel( -1 )
| 00:01:44.210 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:44.220 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 4 ]} Attach:[4] Exit Test Step ts_CRLC_Rel
Attach:[5] Enter Test Step ts_SS_RB1_ToRB4_Cfg( )
| 00:01:44.220 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:44.240 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 1 ]} 00:01:44.240 - Primitive: CRLC_Config_REQ Send event:[3] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:44.250 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[4] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 2 ]} 00:01:44.250 - Primitive: CRLC_Config_REQ Send event:[5] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:44.270 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[6] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 3 ]} 00:01:44.270 - Primitive: CRLC_Config_REQ Send event:[7] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:44.290 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[8] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 4 ]} Attach:[5] Exit Test Step ts_SS_RB1_ToRB4_Cfg
Attach:[10] Exit Test Step ts_CRLC_RelReconfSRB
Attach:[11] Enter Test Step ts_SetCellCfg( 6 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 6 )
| Assignment:[14] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Assignment:[2] cellConfig := cell_FACH_NoConn Attach:[3] Enter Test Step ts_SaveCellInfo( 6 )
| Assignment:[14] tcv_CellInfoG := (view Assignment) Attach:[3] Exit Test Step ts_SaveCellInfo
Attach:[11] Exit Test Step ts_SetCellCfg
Attach:[4] Exit Test Step ts_RRC_ConnRel::lt_RestartCRLC_ForNextConnection
Attach:[5] Enter Test Step ts_SS_ResetSecurityKey( )
| Assignment:[1] tcv_CellIndInfo := (view Assignment) Assignment:[5] cipheringAlgorithmCapability := '0000000000000001'B Attach:[5] Exit Test Step ts_SS_ResetSecurityKey
Attach:[42] Exit Test Step ts_RRC_ConnRel
Attach:[4] Exit Test Step ts_NAS_UpdateRegistration::lt_RRC_ConnRel
Attach:[2] Exit Test Step ts_NAS_UpdateRegistration
Attach:[25] Exit Test Step ts_UpdateRegistration
Assignment:[26] tcv_TestBody := GcFALSE Attach:[8] Exit Test Step tc_6_1_1_7::lt_LocalTest
Attach:[9] Enter Test Step po_ConnectionAndSS_Rels( )
| Attach:[1] Enter Test Step po_ConnectionAndSS_Rels::lt_ReleaseCell( 0 )
| Attach:[9] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[9] Exit Test Step ts_SetTmpCellInfo
Attach:[11] Enter Test Step po_ConnectionAndSS_Rel( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[3] Enter Test Step po_ConnectionAndSS_Rel::lt_Send_RRC_ConnectionRelease( 0 )
| Attach:[3] Exit Test Step po_ConnectionAndSS_Rel::lt_Send_RRC_ConnectionRelease
Attach:[4] Enter Test Step ts_SS_Rel( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[74] Enter Test Step ts_SS_Rel::lt_ReleaseCommonCh( 0 )
| Attach:[328] Enter Test Step ts_CRLC_Rel( 0 )
| 00:01:44.290 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:44.300 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: 0 ]} Attach:[328] Exit Test Step ts_CRLC_Rel
Attach:[329] Enter Test Step ts_CMAC_Rel( 0 )
| 00:01:44.300 - Primitive: CMAC_Config_REQ Send event:[1] CMAC ! CMAC_Config_REQ = PDU (view PDU) 00:01:44.320 - Primitive: CMAC_Config_CNF begin "ca_CMAC_CfgCnf" of type CMAC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 8 against 8 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_CfgCnf" of type CMAC_Config_CNF Receive event:[2] CMAC ? CMAC_Config_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 8 ]} Attach:[329] Exit Test Step ts_CMAC_Rel
Attach:[330] Enter Test Step ts_CPHY_TrChRelNonDch( 0 )
| 00:01:44.320 - Primitive: CPHY_TrCH_Release_REQ Send event:[1] CPHY ! CPHY_TrCH_Release_REQ = PDU (view PDU) 00:01:44.330 - Primitive: CPHY_TrCH_Release_CNF begin "ca_PHY_RelCnf" of type CPHY_TrCH_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 8 against 8 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_PHY_RelCnf" of type CPHY_TrCH_Release_CNF Receive event:[2] CPHY ? CPHY_TrCH_Release_CNF = PDU (view PDU) Attach:[330] Exit Test Step ts_CPHY_TrChRelNonDch
Attach:[331] Enter Test Step ts_SS_StopRL( 0 )
| 00:01:44.330 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 7 ]} 00:01:44.350 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 7 against 7 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 7 ]} Attach:[331] Exit Test Step ts_SS_StopRL
Attach:[332] Enter Test Step ts_SS_StopRL( 0 )
| 00:01:44.350 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 8 ]} 00:01:44.360 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 8 against 8 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 8 ]} Attach:[332] Exit Test Step ts_SS_StopRL
Attach:[333] Enter Test Step ts_CRLC_Rel( 0 )
| 00:01:44.360 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:44.380 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -2 against -2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -2 ]} Attach:[333] Exit Test Step ts_CRLC_Rel
Attach:[334] Enter Test Step ts_CMAC_Rel( 0 )
| 00:01:44.380 - Primitive: CMAC_Config_REQ Send event:[1] CMAC ! CMAC_Config_REQ = PDU (view PDU) 00:01:44.390 - Primitive: CMAC_Config_CNF begin "ca_CMAC_CfgCnf" of type CMAC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 5 against 5 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_CfgCnf" of type CMAC_Config_CNF Receive event:[2] CMAC ? CMAC_Config_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 5 ]} Attach:[334] Exit Test Step ts_CMAC_Rel
Attach:[335] Enter Test Step ts_CPHY_TrChRelNonDch( 0 )
| 00:01:44.390 - Primitive: CPHY_TrCH_Release_REQ Send event:[1] CPHY ! CPHY_TrCH_Release_REQ = PDU (view PDU) 00:01:44.410 - Primitive: CPHY_TrCH_Release_CNF begin "ca_PHY_RelCnf" of type CPHY_TrCH_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 5 against 5 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_PHY_RelCnf" of type CPHY_TrCH_Release_CNF Receive event:[2] CPHY ? CPHY_TrCH_Release_CNF = PDU (view PDU) Attach:[335] Exit Test Step ts_CPHY_TrChRelNonDch
Attach:[336] Enter Test Step ts_SS_StopRL( 0 )
| 00:01:44.410 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 6 ]} 00:01:44.440 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 6 ]} Attach:[336] Exit Test Step ts_SS_StopRL
Attach:[337] Enter Test Step ts_SS_StopRL( 0 )
| 00:01:44.440 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 5 ]} 00:01:44.460 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 5 against 5 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 5 ]} Attach:[337] Exit Test Step ts_SS_StopRL
Attach:[74] Exit Test Step ts_SS_Rel::lt_ReleaseCommonCh
Attach:[75] Enter Test Step ts_SS_Rel::lt_Release_BCCH( 0 )
| Attach:[321] Enter Test Step ts_CRLC_Rel( 0 )
| 00:01:44.460 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:44.470 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} Attach:[321] Exit Test Step ts_CRLC_Rel
Attach:[322] Enter Test Step ts_CMAC_Rel( 0 )
| 00:01:44.470 - Primitive: CMAC_Config_REQ Send event:[1] CMAC ! CMAC_Config_REQ = PDU (view PDU) 00:01:44.490 - Primitive: CMAC_Config_CNF begin "ca_CMAC_CfgCnf" of type CMAC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_CfgCnf" of type CMAC_Config_CNF Receive event:[2] CMAC ? CMAC_Config_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 4 ]} Attach:[322] Exit Test Step ts_CMAC_Rel
Attach:[323] Enter Test Step ts_CPHY_TrChRelNonDch( 0 )
| 00:01:44.490 - Primitive: CPHY_TrCH_Release_REQ Send event:[1] CPHY ! CPHY_TrCH_Release_REQ = PDU (view PDU) 00:01:44.500 - Primitive: CPHY_TrCH_Release_CNF begin "ca_PHY_RelCnf" of type CPHY_TrCH_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_PHY_RelCnf" of type CPHY_TrCH_Release_CNF Receive event:[2] CPHY ? CPHY_TrCH_Release_CNF = PDU (view PDU) Attach:[323] Exit Test Step ts_CPHY_TrChRelNonDch
Attach:[324] Enter Test Step ts_SS_StopRL( 0 )
| 00:01:44.500 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 2 ]} 00:01:44.520 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 2 ]} Attach:[324] Exit Test Step ts_SS_StopRL
Attach:[325] Enter Test Step ts_SS_StopRL( 0 )
| 00:01:44.520 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 1 ]} 00:01:44.540 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 1 ]} Attach:[325] Exit Test Step ts_SS_StopRL
Attach:[326] Enter Test Step ts_SS_StopRL( 0 )
| 00:01:44.540 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 4 ]} 00:01:44.550 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 4 ]} Attach:[326] Exit Test Step ts_SS_StopRL
Attach:[327] Enter Test Step ts_SS_StopRL( 0 )
| 00:01:44.550 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 0 ]} 00:01:44.570 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 0 ]} Attach:[327] Exit Test Step ts_SS_StopRL
Attach:[75] Exit Test Step ts_SS_Rel::lt_Release_BCCH
Attach:[76] Enter Test Step ts_SetCellCfg( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Assignment:[2] cellConfig := cell_NotConfigured Attach:[3] Enter Test Step ts_SaveCellInfo( 0 )
| Assignment:[2] tcv_CellInfoA := (view Assignment) Attach:[3] Exit Test Step ts_SaveCellInfo
Attach:[76] Exit Test Step ts_SetCellCfg
Attach:[4] Exit Test Step ts_SS_Rel
Attach:[11] Exit Test Step po_ConnectionAndSS_Rel
Attach:[1] Exit Test Step po_ConnectionAndSS_Rels::lt_ReleaseCell
Attach:[2] Enter Test Step po_ConnectionAndSS_Rels::lt_ReleaseCell( 1 )
| Attach:[9] Enter Test Step ts_SetTmpCellInfo( 1 )
| Assignment:[4] tcv_TmpCellInfo := (view Assignment) Attach:[9] Exit Test Step ts_SetTmpCellInfo
Attach:[2] Exit Test Step po_ConnectionAndSS_Rels::lt_ReleaseCell
Attach:[3] Enter Test Step po_ConnectionAndSS_Rels::lt_ReleaseCell( 2 )
| Attach:[9] Enter Test Step ts_SetTmpCellInfo( 2 )
| Assignment:[6] tcv_TmpCellInfo := (view Assignment) Attach:[9] Exit Test Step ts_SetTmpCellInfo
Attach:[3] Exit Test Step po_ConnectionAndSS_Rels::lt_ReleaseCell
Attach:[4] Enter Test Step po_ConnectionAndSS_Rels::lt_ReleaseCell( 3 )
| Attach:[9] Enter Test Step ts_SetTmpCellInfo( 3 )
| Assignment:[8] tcv_TmpCellInfo := (view Assignment) Attach:[9] Exit Test Step ts_SetTmpCellInfo
Attach:[11] Enter Test Step po_ConnectionAndSS_Rel( 3 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 3 )
| Assignment:[8] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[3] Enter Test Step po_ConnectionAndSS_Rel::lt_Send_RRC_ConnectionRelease( 3 )
| Attach:[3] Exit Test Step po_ConnectionAndSS_Rel::lt_Send_RRC_ConnectionRelease
Attach:[4] Enter Test Step ts_SS_Rel( 3 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 3 )
| Assignment:[8] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[74] Enter Test Step ts_SS_Rel::lt_ReleaseCommonCh( 3 )
| Attach:[328] Enter Test Step ts_CRLC_Rel( 3 )
| 00:01:44.570 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:44.580 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: 0 ]} Attach:[328] Exit Test Step ts_CRLC_Rel
Attach:[329] Enter Test Step ts_CMAC_Rel( 3 )
| 00:01:44.580 - Primitive: CMAC_Config_REQ Send event:[1] CMAC ! CMAC_Config_REQ = PDU (view PDU) 00:01:44.600 - Primitive: CMAC_Config_CNF begin "ca_CMAC_CfgCnf" of type CMAC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 8 against 8 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_CfgCnf" of type CMAC_Config_CNF Receive event:[2] CMAC ? CMAC_Config_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 8 ]} Attach:[329] Exit Test Step ts_CMAC_Rel
Attach:[330] Enter Test Step ts_CPHY_TrChRelNonDch( 3 )
| 00:01:44.600 - Primitive: CPHY_TrCH_Release_REQ Send event:[1] CPHY ! CPHY_TrCH_Release_REQ = PDU (view PDU) 00:01:44.610 - Primitive: CPHY_TrCH_Release_CNF begin "ca_PHY_RelCnf" of type CPHY_TrCH_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 8 against 8 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_PHY_RelCnf" of type CPHY_TrCH_Release_CNF Receive event:[2] CPHY ? CPHY_TrCH_Release_CNF = PDU (view PDU) Attach:[330] Exit Test Step ts_CPHY_TrChRelNonDch
Attach:[331] Enter Test Step ts_SS_StopRL( 3 )
| 00:01:44.610 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 7 ]} 00:01:44.630 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 7 against 7 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 7 ]} Attach:[331] Exit Test Step ts_SS_StopRL
Attach:[332] Enter Test Step ts_SS_StopRL( 3 )
| 00:01:44.630 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 8 ]} 00:01:44.640 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 8 against 8 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 8 ]} Attach:[332] Exit Test Step ts_SS_StopRL
Attach:[333] Enter Test Step ts_CRLC_Rel( 3 )
| 00:01:44.640 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:44.660 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -2 against -2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -2 ]} Attach:[333] Exit Test Step ts_CRLC_Rel
Attach:[334] Enter Test Step ts_CMAC_Rel( 3 )
| 00:01:44.660 - Primitive: CMAC_Config_REQ Send event:[1] CMAC ! CMAC_Config_REQ = PDU (view PDU) 00:01:44.680 - Primitive: CMAC_Config_CNF begin "ca_CMAC_CfgCnf" of type CMAC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 5 against 5 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_CfgCnf" of type CMAC_Config_CNF Receive event:[2] CMAC ? CMAC_Config_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 5 ]} Attach:[334] Exit Test Step ts_CMAC_Rel
Attach:[335] Enter Test Step ts_CPHY_TrChRelNonDch( 3 )
| 00:01:44.680 - Primitive: CPHY_TrCH_Release_REQ Send event:[1] CPHY ! CPHY_TrCH_Release_REQ = PDU (view PDU) 00:01:44.690 - Primitive: CPHY_TrCH_Release_CNF begin "ca_PHY_RelCnf" of type CPHY_TrCH_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 5 against 5 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_PHY_RelCnf" of type CPHY_TrCH_Release_CNF Receive event:[2] CPHY ? CPHY_TrCH_Release_CNF = PDU (view PDU) Attach:[335] Exit Test Step ts_CPHY_TrChRelNonDch
Attach:[336] Enter Test Step ts_SS_StopRL( 3 )
| 00:01:44.690 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 6 ]} 00:01:44.710 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 6 ]} Attach:[336] Exit Test Step ts_SS_StopRL
Attach:[337] Enter Test Step ts_SS_StopRL( 3 )
| 00:01:44.710 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 5 ]} 00:01:44.720 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 5 against 5 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 5 ]} Attach:[337] Exit Test Step ts_SS_StopRL
Attach:[74] Exit Test Step ts_SS_Rel::lt_ReleaseCommonCh
Attach:[75] Enter Test Step ts_SS_Rel::lt_Release_BCCH( 3 )
| Attach:[321] Enter Test Step ts_CRLC_Rel( 3 )
| 00:01:44.720 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:44.740 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} Attach:[321] Exit Test Step ts_CRLC_Rel
Attach:[322] Enter Test Step ts_CMAC_Rel( 3 )
| 00:01:44.740 - Primitive: CMAC_Config_REQ Send event:[1] CMAC ! CMAC_Config_REQ = PDU (view PDU) 00:01:44.770 - Primitive: CMAC_Config_CNF begin "ca_CMAC_CfgCnf" of type CMAC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_CfgCnf" of type CMAC_Config_CNF Receive event:[2] CMAC ? CMAC_Config_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 4 ]} Attach:[322] Exit Test Step ts_CMAC_Rel
Attach:[323] Enter Test Step ts_CPHY_TrChRelNonDch( 3 )
| 00:01:44.770 - Primitive: CPHY_TrCH_Release_REQ Send event:[1] CPHY ! CPHY_TrCH_Release_REQ = PDU (view PDU) 00:01:44.790 - Primitive: CPHY_TrCH_Release_CNF begin "ca_PHY_RelCnf" of type CPHY_TrCH_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_PHY_RelCnf" of type CPHY_TrCH_Release_CNF Receive event:[2] CPHY ? CPHY_TrCH_Release_CNF = PDU (view PDU) Attach:[323] Exit Test Step ts_CPHY_TrChRelNonDch
Attach:[324] Enter Test Step ts_SS_StopRL( 3 )
| 00:01:44.790 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 2 ]} 00:01:44.800 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 2 ]} Attach:[324] Exit Test Step ts_SS_StopRL
Attach:[325] Enter Test Step ts_SS_StopRL( 3 )
| 00:01:44.800 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 1 ]} 00:01:44.820 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 1 ]} Attach:[325] Exit Test Step ts_SS_StopRL
Attach:[326] Enter Test Step ts_SS_StopRL( 3 )
| 00:01:44.820 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 4 ]} 00:01:44.830 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 4 ]} Attach:[326] Exit Test Step ts_SS_StopRL
Attach:[327] Enter Test Step ts_SS_StopRL( 3 )
| 00:01:44.830 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 0 ]} 00:01:44.850 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 0 ]} Attach:[327] Exit Test Step ts_SS_StopRL
Attach:[75] Exit Test Step ts_SS_Rel::lt_Release_BCCH
Attach:[76] Enter Test Step ts_SetCellCfg( 3 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 3 )
| Assignment:[8] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Assignment:[2] cellConfig := cell_NotConfigured Attach:[3] Enter Test Step ts_SaveCellInfo( 3 )
| Assignment:[8] tcv_CellInfoD := (view Assignment) Attach:[3] Exit Test Step ts_SaveCellInfo
Attach:[76] Exit Test Step ts_SetCellCfg
Attach:[4] Exit Test Step ts_SS_Rel
Attach:[11] Exit Test Step po_ConnectionAndSS_Rel
Attach:[4] Exit Test Step po_ConnectionAndSS_Rels::lt_ReleaseCell
Attach:[5] Enter Test Step po_ConnectionAndSS_Rels::lt_ReleaseCell( 4 )
| Attach:[9] Enter Test Step ts_SetTmpCellInfo( 4 )
| Assignment:[10] tcv_TmpCellInfo := (view Assignment) Attach:[9] Exit Test Step ts_SetTmpCellInfo
Attach:[5] Exit Test Step po_ConnectionAndSS_Rels::lt_ReleaseCell
Attach:[6] Enter Test Step po_ConnectionAndSS_Rels::lt_ReleaseCell( 5 )
| Attach:[9] Enter Test Step ts_SetTmpCellInfo( 5 )
| Assignment:[12] tcv_TmpCellInfo := (view Assignment) Attach:[9] Exit Test Step ts_SetTmpCellInfo
Attach:[6] Exit Test Step po_ConnectionAndSS_Rels::lt_ReleaseCell
Attach:[7] Enter Test Step po_ConnectionAndSS_Rels::lt_ReleaseCell( 6 )
| Attach:[9] Enter Test Step ts_SetTmpCellInfo( 6 )
| Assignment:[14] tcv_TmpCellInfo := (view Assignment) Attach:[9] Exit Test Step ts_SetTmpCellInfo
Attach:[11] Enter Test Step po_ConnectionAndSS_Rel( 6 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 6 )
| Assignment:[14] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[3] Enter Test Step po_ConnectionAndSS_Rel::lt_Send_RRC_ConnectionRelease( 6 )
| Attach:[3] Exit Test Step po_ConnectionAndSS_Rel::lt_Send_RRC_ConnectionRelease
Attach:[4] Enter Test Step ts_SS_Rel( 6 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 6 )
| Assignment:[14] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[12] Enter Test Step ts_SS_Rel::lt_RelSRB1_4( 6 )
| Attach:[338] Enter Test Step ts_CRLC_Rel( -1 )
| 00:01:44.850 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:44.860 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 1 ]} Attach:[338] Exit Test Step ts_CRLC_Rel
Attach:[339] Enter Test Step ts_CRLC_Rel( -1 )
| 00:01:44.860 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:44.880 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 2 ]} Attach:[339] Exit Test Step ts_CRLC_Rel
Attach:[340] Enter Test Step ts_CRLC_Rel( -1 )
| 00:01:44.880 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:44.890 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 3 ]} Attach:[340] Exit Test Step ts_CRLC_Rel
Attach:[341] Enter Test Step ts_CRLC_Rel( -1 )
| 00:01:44.890 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:44.910 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 4 ]} Attach:[341] Exit Test Step ts_CRLC_Rel
Attach:[12] Exit Test Step ts_SS_Rel::lt_RelSRB1_4
Attach:[13] Enter Test Step ts_CRLC_Rel( -1 )
| 00:01:44.910 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:44.930 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 20 against 20 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 20 ]} Attach:[13] Exit Test Step ts_CRLC_Rel
Attach:[14] Enter Test Step ts_CRLC_Rel( 6 )
| 00:01:44.930 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:44.940 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -3 against -3 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: 6 , routingInfo: [rB_Identity: -3 ]} Attach:[14] Exit Test Step ts_CRLC_Rel
Attach:[15] Enter Test Step ts_SS_Rel::lt_ReleaseCommonCh( 6 )
| Attach:[328] Enter Test Step ts_CRLC_Rel( 6 )
| 00:01:44.940 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:44.960 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: 6 , routingInfo: [rB_Identity: 0 ]} Attach:[328] Exit Test Step ts_CRLC_Rel
Attach:[329] Enter Test Step ts_CMAC_Rel( 6 )
| 00:01:44.960 - Primitive: CMAC_Config_REQ Send event:[1] CMAC ! CMAC_Config_REQ = PDU (view PDU) 00:01:44.990 - Primitive: CMAC_Config_CNF begin "ca_CMAC_CfgCnf" of type CMAC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 8 against 8 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_CfgCnf" of type CMAC_Config_CNF Receive event:[2] CMAC ? CMAC_Config_CNF = PDU: { cellId: 6 , routingInfo: [physicalChannelIdentity: 8 ]} Attach:[329] Exit Test Step ts_CMAC_Rel
Attach:[330] Enter Test Step ts_CPHY_TrChRelNonDch( 6 )
| 00:01:44.990 - Primitive: CPHY_TrCH_Release_REQ Send event:[1] CPHY ! CPHY_TrCH_Release_REQ = PDU (view PDU) 00:01:45.000 - Primitive: CPHY_TrCH_Release_CNF begin "ca_PHY_RelCnf" of type CPHY_TrCH_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 8 against 8 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_PHY_RelCnf" of type CPHY_TrCH_Release_CNF Receive event:[2] CPHY ? CPHY_TrCH_Release_CNF = PDU (view PDU) Attach:[330] Exit Test Step ts_CPHY_TrChRelNonDch
Attach:[331] Enter Test Step ts_SS_StopRL( 6 )
| 00:01:45.000 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 6 , routingInfo: [physicalChannelIdentity: 7 ]} 00:01:45.020 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 7 against 7 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 6 , routingInfo: [physicalChannelIdentity: 7 ]} Attach:[331] Exit Test Step ts_SS_StopRL
Attach:[332] Enter Test Step ts_SS_StopRL( 6 )
| 00:01:45.020 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 6 , routingInfo: [physicalChannelIdentity: 8 ]} 00:01:45.040 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 8 against 8 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 6 , routingInfo: [physicalChannelIdentity: 8 ]} Attach:[332] Exit Test Step ts_SS_StopRL
Attach:[333] Enter Test Step ts_CRLC_Rel( 6 )
| 00:01:45.040 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:45.050 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -2 against -2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: 6 , routingInfo: [rB_Identity: -2 ]} Attach:[333] Exit Test Step ts_CRLC_Rel
Attach:[334] Enter Test Step ts_CMAC_Rel( 6 )
| 00:01:45.050 - Primitive: CMAC_Config_REQ Send event:[1] CMAC ! CMAC_Config_REQ = PDU (view PDU) 00:01:45.070 - Primitive: CMAC_Config_CNF begin "ca_CMAC_CfgCnf" of type CMAC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 5 against 5 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_CfgCnf" of type CMAC_Config_CNF Receive event:[2] CMAC ? CMAC_Config_CNF = PDU: { cellId: 6 , routingInfo: [physicalChannelIdentity: 5 ]} Attach:[334] Exit Test Step ts_CMAC_Rel
Attach:[335] Enter Test Step ts_CPHY_TrChRelNonDch( 6 )
| 00:01:45.070 - Primitive: CPHY_TrCH_Release_REQ Send event:[1] CPHY ! CPHY_TrCH_Release_REQ = PDU (view PDU) 00:01:45.080 - Primitive: CPHY_TrCH_Release_CNF begin "ca_PHY_RelCnf" of type CPHY_TrCH_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 5 against 5 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_PHY_RelCnf" of type CPHY_TrCH_Release_CNF Receive event:[2] CPHY ? CPHY_TrCH_Release_CNF = PDU (view PDU) Attach:[335] Exit Test Step ts_CPHY_TrChRelNonDch
Attach:[336] Enter Test Step ts_SS_StopRL( 6 )
| 00:01:45.080 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 6 , routingInfo: [physicalChannelIdentity: 6 ]} 00:01:45.100 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 6 , routingInfo: [physicalChannelIdentity: 6 ]} Attach:[336] Exit Test Step ts_SS_StopRL
Attach:[337] Enter Test Step ts_SS_StopRL( 6 )
| 00:01:45.100 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 6 , routingInfo: [physicalChannelIdentity: 5 ]} 00:01:45.110 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 5 against 5 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 6 , routingInfo: [physicalChannelIdentity: 5 ]} Attach:[337] Exit Test Step ts_SS_StopRL
Attach:[15] Exit Test Step ts_SS_Rel::lt_ReleaseCommonCh
Attach:[16] Enter Test Step ts_SS_Rel::lt_Release_BCCH( 6 )
| Attach:[321] Enter Test Step ts_CRLC_Rel( 6 )
| 00:01:45.110 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:45.130 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: 6 , routingInfo: [rB_Identity: -1 ]} Attach:[321] Exit Test Step ts_CRLC_Rel
Attach:[322] Enter Test Step ts_CMAC_Rel( 6 )
| 00:01:45.130 - Primitive: CMAC_Config_REQ Send event:[1] CMAC ! CMAC_Config_REQ = PDU (view PDU) 00:01:45.160 - Primitive: CMAC_Config_CNF begin "ca_CMAC_CfgCnf" of type CMAC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_CfgCnf" of type CMAC_Config_CNF Receive event:[2] CMAC ? CMAC_Config_CNF = PDU: { cellId: 6 , routingInfo: [physicalChannelIdentity: 4 ]} Attach:[322] Exit Test Step ts_CMAC_Rel
Attach:[323] Enter Test Step ts_CPHY_TrChRelNonDch( 6 )
| 00:01:45.160 - Primitive: CPHY_TrCH_Release_REQ Send event:[1] CPHY ! CPHY_TrCH_Release_REQ = PDU (view PDU) 00:01:45.180 - Primitive: CPHY_TrCH_Release_CNF begin "ca_PHY_RelCnf" of type CPHY_TrCH_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_PHY_RelCnf" of type CPHY_TrCH_Release_CNF Receive event:[2] CPHY ? CPHY_TrCH_Release_CNF = PDU (view PDU) Attach:[323] Exit Test Step ts_CPHY_TrChRelNonDch
Attach:[324] Enter Test Step ts_SS_StopRL( 6 )
| 00:01:45.180 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 6 , routingInfo: [physicalChannelIdentity: 2 ]} 00:01:45.190 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 6 , routingInfo: [physicalChannelIdentity: 2 ]} Attach:[324] Exit Test Step ts_SS_StopRL
Attach:[325] Enter Test Step ts_SS_StopRL( 6 )
| 00:01:45.190 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 6 , routingInfo: [physicalChannelIdentity: 1 ]} 00:01:45.210 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 6 , routingInfo: [physicalChannelIdentity: 1 ]} Attach:[325] Exit Test Step ts_SS_StopRL
Attach:[326] Enter Test Step ts_SS_StopRL( 6 )
| 00:01:45.210 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 6 , routingInfo: [physicalChannelIdentity: 4 ]} 00:01:45.220 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 6 , routingInfo: [physicalChannelIdentity: 4 ]} Attach:[326] Exit Test Step ts_SS_StopRL
Attach:[327] Enter Test Step ts_SS_StopRL( 6 )
| 00:01:45.220 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 6 , routingInfo: [physicalChannelIdentity: 0 ]} 00:01:45.240 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 6 , routingInfo: [physicalChannelIdentity: 0 ]} Attach:[327] Exit Test Step ts_SS_StopRL
Attach:[16] Exit Test Step ts_SS_Rel::lt_Release_BCCH
Attach:[17] Enter Test Step ts_SetCellCfg( 6 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 6 )
| Assignment:[14] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Assignment:[2] cellConfig := cell_NotConfigured Attach:[3] Enter Test Step ts_SaveCellInfo( 6 )
| Assignment:[14] tcv_CellInfoG := (view Assignment) Attach:[3] Exit Test Step ts_SaveCellInfo
Attach:[17] Exit Test Step ts_SetCellCfg
Attach:[4] Exit Test Step ts_SS_Rel
Attach:[11] Exit Test Step po_ConnectionAndSS_Rel
Attach:[7] Exit Test Step po_ConnectionAndSS_Rels::lt_ReleaseCell
Attach:[8] Enter Test Step po_ConnectionAndSS_Rels::lt_ReleaseCell( 7 )
| Attach:[9] Enter Test Step ts_SetTmpCellInfo( 7 )
| Assignment:[16] tcv_TmpCellInfo := (view Assignment) Attach:[9] Exit Test Step ts_SetTmpCellInfo
Attach:[8] Exit Test Step po_ConnectionAndSS_Rels::lt_ReleaseCell
Attach:[9] Exit Test Step po_ConnectionAndSS_Rels
CancelTimer:[(implicit)] t_Guard [300] 300 s