| RRC_wk26-tc_8_4_1_25cs_2004-07-14_14.24.25

TTCN Test Step: ts_CountConfiguredCell::lt_CheckOneCell

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 100,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 1,
      nmo: '00'O,
      ura_Identity: '0000000000000001'B,
      t3212: '1E'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NotConfigured,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 0,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }
    )

TTCN Test Step: ts_CountConfiguredCell::lt_CheckOneCell

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 150,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 1,
      nmo: '00'O,
      ura_Identity: '0000000000000001'B,
      t3212: '1E'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NotConfigured,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 1000,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }
    )

TTCN Test Step: ts_CountConfiguredCell::lt_CheckOneCell

(To search, click here and then press Ctrl+F)

    {
      cellId: 2,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 200,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 1,
      nmo: '00'O,
      ura_Identity: '0000000000000010'B,
      t3212: '1E'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NotConfigured,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 2000,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }
    )

TTCN Test Step: ts_CountConfiguredCell::lt_CheckOneCell

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10837
          }
        ]
      },
      attenuationLevel: 30,
      priScrmCode: 250,
      powerpCPICH: -55,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 321,
      sfnOffset: 3000,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 1,
      nmo: '00'O,
      ura_Identity: '0000000000000010'B,
      t3212: '1E'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NotConfigured,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 0,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }
    )

TTCN Test Step: ts_CountConfiguredCell::lt_CheckOneCell

(To search, click here and then press Ctrl+F)

    {
      cellId: 4,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10837
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 300,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 833,
      sfnOffset: 3000,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 1,
      nmo: '00'O,
      ura_Identity: '0000000000000011'B,
      t3212: '1E'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NotConfigured,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 4000,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }
    )

TTCN Test Step: ts_CountConfiguredCell::lt_CheckOneCell

(To search, click here and then press Ctrl+F)

    {
      cellId: 5,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10837
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 350,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 6577,
      sfnOffset: 678,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 1,
      nmo: '00'O,
      ura_Identity: '0000000000000011'B,
      t3212: '1E'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NotConfigured,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 5000,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }
    )

TTCN Test Step: ts_CountConfiguredCell::lt_CheckOneCell

(To search, click here and then press Ctrl+F)

    {
      cellId: 6,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 400,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 7253,
      sfnOffset: 1356,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 1,
      nmo: '00'O,
      ura_Identity: '0000000000000100'B,
      t3212: '1E'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NotConfigured,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 6000,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }
    )

TTCN Test Step: ts_CountConfiguredCell::lt_CheckOneCell

(To search, click here and then press Ctrl+F)

    {
      cellId: 7,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 450,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 4351,
      sfnOffset: 2034,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 1,
      nmo: '00'O,
      ura_Identity: '0000000000000100'B,
      t3212: '1E'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NotConfigured,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 7000,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }
    )

TTCN Test Step: ts_CountConfiguredCell::lt_CheckOneCell

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 100,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 1,
      nmo: '00'O,
      ura_Identity: '0000000000000001'B,
      t3212: '1E'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NotConfigured,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 0,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }
    )

TTCN Test Step: ts_CountConfiguredCell::lt_CheckOneCell

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 150,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 1,
      nmo: '00'O,
      ura_Identity: '0000000000000001'B,
      t3212: '1E'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NotConfigured,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 1000,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }
    )

TTCN Test Step: ts_CountConfiguredCell::lt_CheckOneCell

(To search, click here and then press Ctrl+F)

    {
      cellId: 2,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 200,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 1,
      nmo: '00'O,
      ura_Identity: '0000000000000010'B,
      t3212: '1E'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NotConfigured,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 2000,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }
    )

TTCN Test Step: ts_CountConfiguredCell::lt_CheckOneCell

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10837
          }
        ]
      },
      attenuationLevel: 30,
      priScrmCode: 250,
      powerpCPICH: -55,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 321,
      sfnOffset: 3000,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 1,
      nmo: '00'O,
      ura_Identity: '0000000000000010'B,
      t3212: '1E'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NotConfigured,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 0,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }
    )

TTCN Test Step: ts_CountConfiguredCell::lt_CheckOneCell

(To search, click here and then press Ctrl+F)

    {
      cellId: 4,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10837
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 300,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 833,
      sfnOffset: 3000,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 1,
      nmo: '00'O,
      ura_Identity: '0000000000000011'B,
      t3212: '1E'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NotConfigured,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 4000,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }
    )

TTCN Test Step: ts_CountConfiguredCell::lt_CheckOneCell

(To search, click here and then press Ctrl+F)

    {
      cellId: 5,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10837
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 350,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 6577,
      sfnOffset: 678,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 1,
      nmo: '00'O,
      ura_Identity: '0000000000000011'B,
      t3212: '1E'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NotConfigured,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 5000,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }
    )

TTCN Test Step: ts_CountConfiguredCell::lt_CheckOneCell

(To search, click here and then press Ctrl+F)

    {
      cellId: 6,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 400,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 7253,
      sfnOffset: 1356,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 1,
      nmo: '00'O,
      ura_Identity: '0000000000000100'B,
      t3212: '1E'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NotConfigured,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 6000,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }
    )

TTCN Test Step: ts_CountConfiguredCell::lt_CheckOneCell

(To search, click here and then press Ctrl+F)

    {
      cellId: 7,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 450,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 4351,
      sfnOffset: 2034,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 1,
      nmo: '00'O,
      ura_Identity: '0000000000000100'B,
      t3212: '1E'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NotConfigured,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 7000,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }
    )

TTCN Test Step: ts_InitializeSIB2AndSIB18

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 100,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 1,
      nmo: '00'O,
      ura_Identity: '0000000000000001'B,
      t3212: '1E'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB_NoConn,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 0,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }
    )

TTCN Test Step: ts_SendSIB1_LongNeighCellInfo

(To search, click here and then press Ctrl+F)

    {
      cn_CommonGSM_MAP_NAS_SysInfo: '0001'O,
      cn_DomainSysInfoList:
      [
        {
          cn_DomainIdentity: ps_domain,
          cn_Type:
          [
            gsm_MAP: '0500'O
          ],
          cn_DRX_CycleLengthCoeff: 7
        },

        {
          cn_DomainIdentity: cs_domain,
          cn_Type:
          [
            gsm_MAP: '1E01'O
          ],
          cn_DRX_CycleLengthCoeff: 7
        }
      ],
      ue_ConnTimersAndConstants:
      {
        t_301: OMIT,
        n_301: OMIT,
        t_302: OMIT,
        n_302: OMIT,
        t_304: OMIT,
        n_304: OMIT,
        t_305: OMIT,
        t_307: OMIT,
        t_308: OMIT,
        t_309: OMIT,
        t_310: OMIT,
        n_310: OMIT,
        t_311: OMIT,
        t_312: OMIT,
        n_312: OMIT,
        t_313: OMIT,
        n_313: OMIT,
        t_314: OMIT,
        t_315: OMIT,
        n_315: OMIT,
        t_316: OMIT,
        t_317: OMIT
      },
      ue_IdleTimersAndConstants:
      {
        t_300: ms4000,
        n_300: 3,
        t_312: 10,
        n_312: s1
      },
      v3a0NonCriticalExtensions: OMIT
    }
    )

TTCN Test Step: ts_SendSIB2_LongNeighCellInfo

(To search, click here and then press Ctrl+F)

    {
      ura_IdentityList:
      [
        '0000000000000001'B
      ],
      nonCriticalExtensions: OMIT
    }
    )

TTCN Test Step: ts_SendSIB3_LongNeighCellInfo

(To search, click here and then press Ctrl+F)

    {
      sib4indicator: GcTRUE,
      cellIdentity: '0000000000000000000000000000'B,
      cellSelectReselectInfo:
      {
        mappingInfo: OMIT,
        cellSelectQualityMeasure:
        [
          cpich_RSCP: NULL
        ],
        modeSpecificInfo:
        [
          fdd:
          {
            s_Intrasearch: 8,
            s_Intersearch: 8,
            s_SearchHCS: OMIT,
            rat_List:
            [
              {
                rat_Identifier: gsm,
                s_SearchRAT: -16,
                s_HCS_RAT: OMIT,
                s_Limit_SearchRAT: 0
              }
            ],
            q_QualMin: -24,
            q_RxlevMin: -40
          }
        ],
        q_Hyst_l_S: 2,
        t_Reselection_S: 0,
        hcs_ServingCellInformation: OMIT,
        maxAllowedUL_TX_Power: 21
      },
      cellAccessRestriction:
      {
        cellBarred:
        [
          notBarred: NULL
        ],
        cellReservedForOperatorUse: notReserved,
        cellReservationExtension: notReserved,
        accessClassBarredList:
        [
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred
        ]
      },
      nonCriticalExtensions: OMIT
    }
    )

TTCN Test Step: ts_SendSIB4_LongNeighCellInfo

(To search, click here and then press Ctrl+F)

    {
      cellIdentity: '0000000000000000000000000000'B,
      cellSelectReselectInfo:
      {
        mappingInfo: OMIT,
        cellSelectQualityMeasure:
        [
          cpich_RSCP: NULL
        ],
        modeSpecificInfo:
        [
          fdd:
          {
            s_Intrasearch: 8,
            s_Intersearch: 8,
            s_SearchHCS: OMIT,
            rat_List:
            [
              {
                rat_Identifier: gsm,
                s_SearchRAT: -16,
                s_HCS_RAT: OMIT,
                s_Limit_SearchRAT: 0
              }
            ],
            q_QualMin: -24,
            q_RxlevMin: -40
          }
        ],
        q_Hyst_l_S: 0,
        t_Reselection_S: 0,
        hcs_ServingCellInformation: OMIT,
        maxAllowedUL_TX_Power: 21
      },
      cellAccessRestriction:
      {
        cellBarred:
        [
          notBarred: NULL
        ],
        cellReservedForOperatorUse: notReserved,
        cellReservationExtension: notReserved,
        accessClassBarredList: OMIT
      },
      nonCriticalExtensions: OMIT
    }
    )

TTCN Test Step: ts_SendSIB5_LongNeighCellInfo

(To search, click here and then press Ctrl+F)

    {
      sib6indicator: GcTRUE,
      pich_PowerOffset: -5,
      modeSpecificInfo:
      [
        fdd:
        {
          aich_PowerOffset: -5
        }
      ],
      primaryCCPCH_Info: OMIT,
      prach_SystemInformationList:
      [
        {
          prach_RACH_Info:
          {
            modeSpecificInfo:
            [
              fdd:
              {
                availableSignatures: '0000000011111111'B,
                availableSF: sfpr64,
                preambleScramblingCodeWordNumber: 0,
                puncturingLimit: pl1,
                availableSubChannelNumbers: '111111111111'B
              }
            ]
          },
          transportChannelIdentity: 15,
          rach_TransportFormatSet:
          [
            commonTransChTFS:
            {
              tti:
              [
                tti20:
                [
                  {
                    rlc_Size:
                    [
                      fdd:
                      {
                        octetModeRLC_SizeInfoType2:
                        [
                          sizeType1: 15
                        ]
                      }
                    ],
                    numberOfTbSizeList:
                    [
                      [
                        one: NULL
                      ]
                    ],
                    logicalChannelList:
                    [
                      configured: NULL
                    ]
                  },

                  {
                    rlc_Size:
                    [
                      fdd:
                      {
                        octetModeRLC_SizeInfoType2:
                        [
                          sizeType2: 3
                        ]
                      }
                    ],
                    numberOfTbSizeList:
                    [
                      [
                        one: NULL
                      ]
                    ],
                    logicalChannelList:
                    [
                      configured: NULL
                    ]
                  }
                ]
              ],
              semistaticTF_Information:
              {
                channelCodingType:
                [
                  convolutional: half
                ],
                rateMatchingAttribute# 150 # crc_Size# crc16
              }
            }
          ]
          # rach_TFCS#
          [
            normalTFCI_Signalling#
            [
              complete#
              {
                ctfcSize#
                [
                  ctfc2Bit#
                  [
                    {
                      ctfc2# 0 # powerOffsetInformation#
                      {
                        gainFactorInformation#
                        [
                          computedGainFactors# 0
                        ]
                        # powerOffsetPp_m# 0
                      }
                    }
                    #
                    {
                      ctfc2# 1 # powerOffsetInformation#
                      {
                        gainFactorInformation#
                        [
                          signalledGainFactors#
                          {
                            modeSpecificInfo#
                            [
                              fdd#
                              {
                                gainFactorBetaC# 11
                              }
                            ]
                            # gainFactorBetaD# 15 # referenceTFC_ID# 0
                          }
                        ]
                        # powerOffsetPp_m# 0
                      }
                    }
                  ]
                ]
              }
            ]
          ]
          # prach_Partitioning#
          [
            fdd#
            [
              {
                accessServiceClass_FDD# OMIT
              }
              #
              {
                accessServiceClass_FDD#
                {
                  availableSignatureStartIndex# 0 # availableSignatureEndIndex# 7 # assignedSubChannelNumber# '1111'B
                }
              }
              #
              {
                accessServiceClass_FDD# OMIT
              }
              #
              {
                accessServiceClass_FDD#
                {
                  availableSignatureStartIndex# 0 # availableSignatureEndIndex# 7 # assignedSubChannelNumber# '1111'B
                }
              }
              #
              {
                accessServiceClass_FDD# OMIT
              }
              #
              {
                accessServiceClass_FDD#
                {
                  availableSignatureStartIndex# 0 # availableSignatureEndIndex# 7 # assignedSubChannelNumber# '1111'B
                }
              }
              #
              {
                accessServiceClass_FDD# OMIT
              }
              #
              {
                accessServiceClass_FDD#
                {
                  availableSignatureStartIndex# 0 # availableSignatureEndIndex# 7 # assignedSubChannelNumber# '1111'B
                }
              }
            ]
          ]
          # persistenceScalingFactorList#
          [
            psf0_9# psf0_9# psf0_9# psf0_9# psf0_9# psf0_9
          ]
          # ac_To_ASC_MappingTable#
          [
            6 # 5 # 4 # 3 # 2 # 1 # 0
          ]
          # modeSpecificInfo#
          [
            fdd#
            {
              primaryCPICH_TX_Power# 31 # constantValue# #10 # prach_PowerOffset#
              {
                powerRampStep# 3 # preambleRetransMax# 4
              }
              # rach_TransmissionParameters#
              {
                mmax# 2 # nb01Min# 3 # nb01Max# 10
              }
              # aich_Info#
              {
                channelisationCode256# 3 # sttd_Indicator# GcFALSE # aich_TransmissionTiming# e0
              }
            }
          ]
        }
      ]
      # sCCPCH_SystemInformationList#
      [
        {
          secondaryCCPCH_Info#
          {
            modeSpecificInfo#
            [
              fdd#
              {
                dummy1# mayBeUsed# dummy2# OMIT# secondaryScramblingCode# OMIT# sttd_Indicator# GcFALSE # sf_AndCodeNumber#
                [
                  sf64# 1
                ]
                # pilotSymbolExistence# GcFALSE # tfci_Existence# GcTRUE # positionFixedOrFlexible# flexible# timingOffset# 0
              }
            ]
          }
          # tfcs#
          [
            normalTFCI_Signalling#
            [
              complete#
              {
                ctfcSize#
                [
                  ctfc4Bit#
                  [
                    {
                      ctfc4# 0 # powerOffsetInformation# OMIT
                    }
                    #
                    {
                      ctfc4# 1 # powerOffsetInformation# OMIT
                    }
                    #
                    {
                      ctfc4# 2 # powerOffsetInformation# OMIT
                    }
                    #
                    {
                      ctfc4# 3 # powerOffsetInformation# OMIT
                    }
                    #
                    {
                      ctfc4# 4 # powerOffsetInformation# OMIT
                    }
                    #
                    {
                      ctfc4# 5 # powerOffsetInformation# OMIT
                    }
                    #
                    {
                      ctfc4# 6 # powerOffsetInformation# OMIT
                    }
                    #
                    {
                      ctfc4# 8 # powerOffsetInformation# OMIT
                    }
                  ]
                ]
              }
            ]
          ]
          # fach_PCH_InformationList#
          [
            {
              transportFormatSet#
              [
                commonTransChTFS#
                {
                  tti#
                  [
                    tti10#
                    [
                      {
                        rlc_Size#
                        [
                          fdd#
                          {
                            octetModeRLC_SizeInfoType2#
                            [
                              sizeType1# 24
                            ]
                          }
                        ]
                        # numberOfTbSizeList#
                        [
                          [
                            zero# NULL
                          ]
                          #
                          [
                            one# NULL
                          ]
                        ]
                        # logicalChannelList#
                        [
                          allSizes# NULL
                        ]
                      }
                    ]
                  ]
                  # semistaticTF_Information#
                  {
                    channelCodingType#
                    [
                      convolutional# half
                    ]
                    # rateMatchingAttribute# 230 # crc_Size# crc16
                  }
                }
              ]
              # transportChannelIdentity# 12 # ctch_Indicator# GcFALSE
            }
            #
            {
              transportFormatSet#
              [
                commonTransChTFS#
                {
                  tti#
                  [
                    tti10#
                    [
                      {
                        rlc_Size#
                        [
                          fdd#
                          {
                            octetModeRLC_SizeInfoType2#
                            [
                              sizeType1# 15
                            ]
                          }
                        ]
                        # numberOfTbSizeList#
                        [
                          [
                            zero# NULL
                          ]
                          #
                          [
                            one# NULL
                          ]
                          #
                          [
                            small# 2
                          ]
                        ]
                        # logicalChannelList#
                        [
                          allSizes# NULL
                        ]
                      }
                    ]
                  ]
                  # semistaticTF_Information#
                  {
                    channelCodingType#
                    [
                      convolutional# half
                    ]
                    # rateMatchingAttribute# 220 # crc_Size# crc16
                  }
                }
              ]
              # transportChannelIdentity# 13 # ctch_Indicator# GcFALSE
            }
            #
            {
              transportFormatSet#
              [
                commonTransChTFS#
                {
                  tti#
                  [
                    tti10#
                    [
                      {
                        rlc_Size#
                        [
                          fdd#
                          {
                            octetModeRLC_SizeInfoType2#
                            [
                              sizeType2# 3
                            ]
                          }
                        ]
                        # numberOfTbSizeList#
                        [
                          [
                            zero# NULL
                          ]
                          #
                          [
                            one# NULL
                          ]
                        ]
                        # logicalChannelList#
                        [
                          allSizes# NULL
                        ]
                      }
                    ]
                  ]
                  # semistaticTF_Information#
                  {
                    channelCodingType#
                    [
                      turbo# NULL
                    ]
                    # rateMatchingAttribute# 130 # crc_Size# crc16
                  }
                }
              ]
              # transportChannelIdentity# 14 # ctch_Indicator# GcFALSE
            }
          ]
          # pich_Info#
          [
            fdd#
            {
              channelisationCode256# 2 # pi_CountPerFrame# e18# sttd_Indicator# GcFALSE
            }
          ]
        }
      ]
      # cbs_DRX_Level1Information# OMIT# nonCriticalExtensions# OMIT
    }
    )

TTCN Test Step: ts_SendSIB6_LongNeighCellInfo

(To search, click here and then press Ctrl+F)

    {
      pich_PowerOffset: -5,
      modeSpecificInfo:
      [
        fdd:
        {
          aich_PowerOffset: -5,
          dummy: OMIT
        }
      ],
      primaryCCPCH_Info: OMIT,
      prach_SystemInformationList: OMIT,
      sCCPCH_SystemInformationList: OMIT,
      cbs_DRX_Level1Information: OMIT,
      nonCriticalExtensions: OMIT
    }
    )

TTCN Test Step: ts_SendSIB7_LongNeighCellInfo

(To search, click here and then press Ctrl+F)

    {
      modeSpecificInfo:
      [
        fdd:
        {
          ul_Interference: -100
        }
      ],
      prach_Information_SIB5_List:
      [
        2
      ],
      prach_Information_SIB6_List:
      [
        2
      ],
      expirationTimeFactor: OMIT,
      nonCriticalExtensions: OMIT
    }
    )

TTCN Test Step: ts_SendSIB7_LongNeighCellInfo::lt_CompleteSIB7OrLastSIB12_CompleteSIB7

(To search, click here and then press Ctrl+F)

    {
      modeSpecificInfo:
      [
        fdd:
        {
          ul_Interference: -100
        }
      ],
      prach_Information_SIB5_List:
      [
        2
      ],
      prach_Information_SIB6_List:
      [
        2
      ],
      expirationTimeFactor: OMIT,
      nonCriticalExtensions: OMIT
    }
    )

TTCN Test Step: ts_SendSIB7_LongNeighCellInfo::lt_ConcatWithSIB3

(To search, click here and then press Ctrl+F)

    {
      modeSpecificInfo:
      [
        fdd:
        {
          ul_Interference: -100
        }
      ],
      prach_Information_SIB5_List:
      [
        2
      ],
      prach_Information_SIB6_List:
      [
        2
      ],
      expirationTimeFactor: OMIT,
      nonCriticalExtensions: OMIT
    }
    )

TTCN Test Step: ts_SendSIB7_LongNeighCellInfo::lt_ConcatWithSIB18

(To search, click here and then press Ctrl+F)

    {
      modeSpecificInfo:
      [
        fdd:
        {
          ul_Interference: -100
        }
      ],
      prach_Information_SIB5_List:
      [
        2
      ],
      prach_Information_SIB6_List:
      [
        2
      ],
      expirationTimeFactor: OMIT,
      nonCriticalExtensions: OMIT
    }
    )

TTCN Test Step: ts_SendSIB7_LongNeighCellInfo::lt_ConcatWithSIB4

(To search, click here and then press Ctrl+F)

    {
      modeSpecificInfo:
      [
        fdd:
        {
          ul_Interference: -100
        }
      ],
      prach_Information_SIB5_List:
      [
        2
      ],
      prach_Information_SIB6_List:
      [
        2
      ],
      expirationTimeFactor: OMIT,
      nonCriticalExtensions: OMIT
    }
    )

TTCN Test Step: ts_SendSIB11_LongNeighCellInfo

(To search, click here and then press Ctrl+F)

    {
      sib12indicator: GcTRUE,
      fach_MeasurementOccasionInfo: OMIT,
      measurementControlSysInfo:
      {
        use_of_HCS:
        [
          hcs_not_used:
          {
            cellSelectQualityMeasure:
            [
              cpich_RSCP:
              {
                intraFreqMeasurementSysInfo:
                {
                  intraFreqMeasurementID: OMIT,
                  intraFreqCellInfoSI_List:
                  {
                    removedIntraFreqCellList: OMIT,
                    newIntraFreqCellList:
                    [
                      {
                        intraFreqCellID: 0,
                        cellInfo:
                        {
                          cellIndividualOffset: OMIT,
                          referenceTimeDifferenceToCell: OMIT,
                          modeSpecificInfo:
                          [
                            fdd:
                            {
                              primaryCPICH_Info:
                              {
                                primaryScramblingCode: 100
                              },
                              primaryCPICH_TX_Power: OMIT,
                              readSFN_Indicator: GcFALSE,
                              tx_DiversityIndicator: GcFALSE
                            }
                          ],
                          cellSelectionReselectionInfo: OMIT
                        }
                      },

                      {
                        intraFreqCellID: 1,
                        cellInfo:
                        {
                          cellIndividualOffset: OMIT,
                          referenceTimeDifferenceToCell: OMIT,
                          modeSpecificInfo:
                          [
                            fdd:
                            {
                              primaryCPICH_Info:
                              {
                                primaryScramblingCode: 150
                              },
                              primaryCPICH_TX_Power: OMIT,
                              readSFN_Indicator: GcTRUE,
                              tx_DiversityIndicator: GcFALSE
                            }
                          ],
                          cellSelectionReselectionInfo: OMIT
                        }
                      },

                      {
                        intraFreqCellID: 2,
                        cellInfo:
                        {
                          cellIndividualOffset: OMIT,
                          referenceTimeDifferenceToCell: OMIT,
                          modeSpecificInfo:
                          [
                            fdd:
                            {
                              primaryCPICH_Info:
                              {
                                primaryScramblingCode: 200
                              },
                              primaryCPICH_TX_Power: OMIT,
                              readSFN_Indicator: GcTRUE,
                              tx_DiversityIndicator: GcFALSE
                            }
                          ],
                          cellSelectionReselectionInfo: OMIT
                        }
                      },

                      {
                        intraFreqCellID: 6,
                        cellInfo:
                        {
                          cellIndividualOffset: OMIT,
                          referenceTimeDifferenceToCell: OMIT,
                          modeSpecificInfo:
                          [
                            fdd:
                            {
                              primaryCPICH_Info:
                              {
                                primaryScramblingCode: 400
                              },
                              primaryCPICH_TX_Power: OMIT,
                              readSFN_Indicator: GcTRUE,
                              tx_DiversityIndicator: GcFALSE
                            }
                          ],
                          cellSelectionReselectionInfo: OMIT
                        }
                      },

                      {
                        intraFreqCellID: 7,
                        cellInfo:
                        {
                          cellIndividualOffset: OMIT,
                          referenceTimeDifferenceToCell: OMIT,
                          modeSpecificInfo:
                          [
                            fdd:
                            {
                              primaryCPICH_Info:
                              {
                                primaryScramblingCode: 450
                              },
                              primaryCPICH_TX_Power: OMIT,
                              readSFN_Indicator: GcTRUE,
                              tx_DiversityIndicator: GcFALSE
                            }
                          ],
                          cellSelectionReselectionInfo: OMIT
                        }
                      }
                    ]
                  },
                  intraFreqMeasQuantity:
                  {
                    filterCoefficient: OMIT,
                    modeSpecificInfo:
                    [
                      fdd:
                      {
                        intraFreqMeasQuantity_FDD: cpich_RSCP
                      }
                    ]
                  },
                  intraFreqReportingQuantityForRACH: OMIT,
                  maxReportedCellsOnRACH: OMIT,
                  reportingInfoForCellDCH:
                  {
                    intraFreqReportingQuantity:
                    {
                      activeSetReportingQuantities:
                      {
                        dummy: noReport,
                        cellIdentity_reportingIndicator: GcTRUE,
                        cellSynchronisationInfoReportingIndicator: GcFALSE,
                        modeSpecificInfo:
                        [
                          fdd:
                          {
                            cpich_Ec_N0_reportingIndicator: GcFALSE,
                            cpich_RSCP_reportingIndicator: GcTRUE,
                            pathloss_reportingIndicator: GcFALSE
                          }
                        ]
                      },
                      monitoredSetReportingQuantities:
                      {
                        dummy: noReport,
                        cellIdentity_reportingIndicator: GcTRUE,
                        cellSynchronisationInfoReportingIndicator: GcTRUE,
                        modeSpecificInfo:
                        [
                          fdd:
                          {
                            cpich_Ec_N0_reportingIndicator: GcFALSE,
                            cpich_RSCP_reportingIndicator: GcTRUE,
                            pathloss_reportingIndicator: GcFALSE
                          }
                        ]
                      },
                      detectedSetReportingQuantities: OMIT
                    },
                    measurementReportingMode:
                    {
                      measurementReportTransferMode: acknowledgedModeRLC,
                      periodicalOrEventTrigger: eventTrigger
                    },
                    reportCriteria:
                    [
                      intraFreqReportingCriteria:
                      {
                        eventCriteriaList:
                        [
                          {
                            event:
                            [
                              e1a:
                              {
                                triggeringCondition: monitoredSetCellsOnly,
                                reportingRange: 5,
                                forbiddenAffectCellList: OMIT,
                                w: 1,
                                reportDeactivationThreshold: t2,
                                reportingAmount: ra4,
                                reportingInterval: ri4
                              }
                            ],
                            hysteresis: 0,
                            timeToTrigger: ttt640,
                            reportingCellStatus:
                            [
                              withinActiveAndOrMonitoredUsedFreq: e3
                            ]
                          },

                          {
                            event:
                            [
                              e1b:
                              {
                                triggeringCondition: activeSetCellsOnly,
                                reportingRange: 5,
                                forbiddenAffectCellList: OMIT,
                                w: 1
                              }
                            ],
                            hysteresis: 0,
                            timeToTrigger: ttt640,
                            reportingCellStatus:
                            [
                              withinActiveAndOrMonitoredUsedFreq: e3
                            ]
                          },

                          {
                            event:
                            [
                              e1c:
                              {
                                replacementActivationThreshold: t3,
                                reportingAmount: ra4,
                                reportingInterval: ri4
                              }
                            ],
                            hysteresis: 0,
                            timeToTrigger: ttt640,
                            reportingCellStatus:
                            [
                              withinActiveAndOrMonitoredUsedFreq: e3
                            ]
                          }
                        ]
                      }
                    ]
                  }
                },
                interFreqMeasurementSysInfo:
                {
                  interFreqCellInfoSI_List:
                  {
                    removedInterFreqCellList: OMIT,
                    newInterFreqCellList:
                    [
                      {
                        interFreqCellID: 3,
                        frequencyInfo:
                        {
                          modeSpecificInfo:
                          [
                            fdd:
                            {
                              uarfcn_UL: OMIT,
                              uarfcn_DL: 10837
                            }
                          ]
                        },
                        cellInfo:
                        {
                          cellIndividualOffset: OMIT,
                          referenceTimeDifferenceToCell: OMIT,
                          modeSpecificInfo:
                          [
                            fdd:
                            {
                              primaryCPICH_Info:
                              {
                                primaryScramblingCode: 250
                              },
                              primaryCPICH_TX_Power: OMIT,
                              readSFN_Indicator: GcFALSE,
                              tx_DiversityIndicator: GcFALSE
                            }
                          ],
                          cellSelectionReselectionInfo: OMIT
                        }
                      },

                      {
                        interFreqCellID: 4,
                        frequencyInfo: OMIT,
                        cellInfo:
                        {
                          cellIndividualOffset: OMIT,
                          referenceTimeDifferenceToCell: OMIT,
                          modeSpecificInfo:
                          [
                            fdd:
                            {
                              primaryCPICH_Info:
                              {
                                primaryScramblingCode: 300
                              },
                              primaryCPICH_TX_Power: OMIT,
                              readSFN_Indicator: GcFALSE,
                              tx_DiversityIndicator: GcFALSE
                            }
                          ],
                          cellSelectionReselectionInfo: OMIT
                        }
                      },

                      {
                        interFreqCellID: 5,
                        frequencyInfo: OMIT,
                        cellInfo:
                        {
                          cellIndividualOffset: OMIT,
                          referenceTimeDifferenceToCell: OMIT,
                          modeSpecificInfo:
                          [
                            fdd:
                            {
                              primaryCPICH_Info:
                              {
                                primaryScramblingCode: 350
                              },
                              primaryCPICH_TX_Power: OMIT,
                              readSFN_Indicator: GcFALSE,
                              tx_DiversityIndicator: GcFALSE
                            }
                          ],
                          cellSelectionReselectionInfo: OMIT
                        }
                      }
                    ]
                  }
                }
              }
            ],
            interRATMeasurementSysInfo: OMIT
          }
        ],
        trafficVolumeMeasSysInfo: OMIT,
        dummy: OMIT
      },
      nonCriticalExtensions: OMIT
    }
    )

TTCN Test Step: ts_SendSIB12_LongNeighCellInfo

(To search, click here and then press Ctrl+F)

    {
      fach_MeasurementOccasionInfo: OMIT,
      measurementControlSysInfo:
      {
        use_of_HCS:
        [
          hcs_not_used:
          {
            cellSelectQualityMeasure:
            [
              cpich_RSCP:
              {
                intraFreqMeasurementSysInfo: OMIT,
                interFreqMeasurementSysInfo: OMIT
              }
            ],
            interRATMeasurementSysInfo: OMIT
          }
        ],
        trafficVolumeMeasSysInfo: OMIT,
        dummy: OMIT
      },
      nonCriticalExtensions: OMIT
    }
    )

TTCN Test Step: ts_SendSIB12_LongNeighCellInfo::lt_CompleteSIB7

(To search, click here and then press Ctrl+F)

    {
      fach_MeasurementOccasionInfo: OMIT,
      measurementControlSysInfo:
      {
        use_of_HCS:
        [
          hcs_not_used:
          {
            cellSelectQualityMeasure:
            [
              cpich_RSCP:
              {
                intraFreqMeasurementSysInfo: OMIT,
                interFreqMeasurementSysInfo: OMIT
              }
            ],
            interRATMeasurementSysInfo: OMIT
          }
        ],
        trafficVolumeMeasSysInfo: OMIT,
        dummy: OMIT
      },
      nonCriticalExtensions: OMIT
    }
    )

TTCN Test Step: ts_SendSIB18_LongNeighCellInfo

(To search, click here and then press Ctrl+F)

    {
      idleModePLMNIdentities:
      {
        plmnsOfIntraFreqCellsList: OMIT,
        plmnsOfInterFreqCellsList: OMIT,
        plmnsOfInterRATCellsList: OMIT
      },
      connectedModePLMNIdentities: OMIT,
      nonCriticalExtensions: OMIT
    }
    )

TTCN Test Step: ts_SendSB1_LongNeighCellInfo

(To search, click here and then press Ctrl+F)

    {
      sib_ReferenceList:
      [
        {
          sib_Type:
          [
            sysInfoType6: 2
          ],
          scheduling:
          {
            scheduling:
            {
              segCount: OMIT,
              sib_Pos:
              [
                rep64: 2
              ],
              sib_PosOffsetInfo: OMIT
            }
          }
        },

        {
          sib_Type:
          [
            sysInfoType7: NULL
          ],
          scheduling:
          {
            scheduling:
            {
              segCount: OMIT,
              sib_Pos:
              [
                rep16: 7
              ],
              sib_PosOffsetInfo: OMIT
            }
          }
        },

        {
          sib_Type:
          [
            sysInfoType11: 2
          ],
          scheduling:
          {
            scheduling:
            {
              segCount: 2,
              sib_Pos:
              [
                rep64: 26
              ],
              sib_PosOffsetInfo:
              [
                so2
              ]
            }
          }
        },

        {
          sib_Type:
          [
            sysInfoType12: 2
          ],
          scheduling:
          {
            scheduling:
            {
              segCount: OMIT,
              sib_Pos:
              [
                rep64: 11
              ],
              sib_PosOffsetInfo: OMIT
            }
          }
        },

        {
          sib_Type:
          [
            sysInfoType18: 2
          ],
          scheduling:
          {
            scheduling:
            {
              segCount: OMIT,
              sib_Pos:
              [
                rep64: 23
              ],
              sib_PosOffsetInfo: OMIT
            }
          }
        }
      ],
      nonCriticalExtensions: OMIT
    }
    )

TTCN Test Step: ts_SendMIB

(To search, click here and then press Ctrl+F)

    {
      mib_ValueTag: 1,
      plmn_Type:
      [
        gsm_MAP:
        {
          plmn_Identity:
          {
            mcc:
            [
              0,
              0,
              1
            ],
            mnc:
            [
              0,
              1
            ]
          }
        }
      ],
      sibSb_ReferenceList:
      [
        {
          sibSb_Type:
          [
            sysInfoTypeSB1: 2
          ],
          scheduling:
          {
            scheduling:
            {
              segCount: OMIT,
              sib_Pos:
              [
                rep16: 1
              ],
              sib_PosOffsetInfo: OMIT
            }
          }
        },

        {
          sibSb_Type:
          [
            sysInfoType1: 2
          ],
          scheduling:
          {
            scheduling:
            {
              segCount: OMIT,
              sib_Pos:
              [
                rep64: 10
              ],
              sib_PosOffsetInfo: OMIT
            }
          }
        },

        {
          sibSb_Type:
          [
            sysInfoType2: 2
          ],
          scheduling:
          {
            scheduling:
            {
              segCount: OMIT,
              sib_Pos:
              [
                rep64: 10
              ],
              sib_PosOffsetInfo: OMIT
            }
          }
        },

        {
          sibSb_Type:
          [
            sysInfoType3: 2
          ],
          scheduling:
          {
            scheduling:
            {
              segCount: OMIT,
              sib_Pos:
              [
                rep64: 7
              ],
              sib_PosOffsetInfo: OMIT
            }
          }
        },

        {
          sibSb_Type:
          [
            sysInfoType4: 2
          ],
          scheduling:
          {
            scheduling:
            {
              segCount: OMIT,
              sib_Pos:
              [
                rep64: 31
              ],
              sib_PosOffsetInfo: OMIT
            }
          }
        },

        {
          sibSb_Type:
          [
            sysInfoType5: 2
          ],
          scheduling:
          {
            scheduling:
            {
              segCount: 3,
              sib_Pos:
              [
                rep64: 18
              ],
              sib_PosOffsetInfo:
              [
                so2,
                so4
              ]
            }
          }
        }
      ],
      nonCriticalExtensions: OMIT
    }
    )

TTCN Test Step: ts_CountConfiguredCell::lt_CheckOneCell

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 100,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 1,
      nmo: '00'O,
      ura_Identity: '0000000000000001'B,
      t3212: '1E'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB_NoConn,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 0,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }
    )

TTCN Test Step: ts_CountConfiguredCell::lt_CheckOneCell

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 150,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 1,
      nmo: '00'O,
      ura_Identity: '0000000000000001'B,
      t3212: '1E'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NotConfigured,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 1000,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }
    )

TTCN Test Step: ts_CountConfiguredCell::lt_CheckOneCell

(To search, click here and then press Ctrl+F)

    {
      cellId: 2,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 200,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 1,
      nmo: '00'O,
      ura_Identity: '0000000000000010'B,
      t3212: '1E'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NotConfigured,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 2000,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }
    )

TTCN Test Step: ts_CountConfiguredCell::lt_CheckOneCell

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10837
          }
        ]
      },
      attenuationLevel: 30,
      priScrmCode: 250,
      powerpCPICH: -55,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 321,
      sfnOffset: 3000,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 1,
      nmo: '00'O,
      ura_Identity: '0000000000000010'B,
      t3212: '1E'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NotConfigured,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 0,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }
    )

TTCN Test Step: ts_CountConfiguredCell::lt_CheckOneCell

(To search, click here and then press Ctrl+F)

    {
      cellId: 4,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10837
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 300,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 833,
      sfnOffset: 3000,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 1,
      nmo: '00'O,
      ura_Identity: '0000000000000011'B,
      t3212: '1E'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NotConfigured,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 4000,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }
    )

TTCN Test Step: ts_CountConfiguredCell::lt_CheckOneCell

(To search, click here and then press Ctrl+F)

    {
      cellId: 5,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10837
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 350,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 6577,
      sfnOffset: 678,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 1,
      nmo: '00'O,
      ura_Identity: '0000000000000011'B,
      t3212: '1E'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NotConfigured,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 5000,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }
    )

TTCN Test Step: ts_CountConfiguredCell::lt_CheckOneCell

(To search, click here and then press Ctrl+F)

    {
      cellId: 6,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 400,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 7253,
      sfnOffset: 1356,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 1,
      nmo: '00'O,
      ura_Identity: '0000000000000100'B,
      t3212: '1E'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NotConfigured,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 6000,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }
    )

TTCN Test Step: ts_CountConfiguredCell::lt_CheckOneCell

(To search, click here and then press Ctrl+F)

    {
      cellId: 7,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 450,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 4351,
      sfnOffset: 2034,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 1,
      nmo: '00'O,
      ura_Identity: '0000000000000100'B,
      t3212: '1E'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NotConfigured,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 7000,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }
    )

TTCN Test Step: ts_CountConfiguredCell::lt_CheckOneCell

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 100,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 1,
      nmo: '00'O,
      ura_Identity: '0000000000000001'B,
      t3212: '1E'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_DCH_StandAloneSRB_NoConn,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 0,
      DL_DPCH_SHO: GcTRUE,
      UL_DPCH_SHO: GcTRUE,
      dl_DPCH_2ndScrCode: 1
    }
    )

TTCN Test Step: ts_CountConfiguredCell::lt_CheckOneCell

(To search, click here and then press Ctrl+F)

    {
      cellId: 1,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 150,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 1,
      nmo: '00'O,
      ura_Identity: '0000000000000001'B,
      t3212: '1E'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NotConfigured,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 1000,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }
    )

TTCN Test Step: ts_CountConfiguredCell::lt_CheckOneCell

(To search, click here and then press Ctrl+F)

    {
      cellId: 2,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 200,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 0,
      sfnOffset: 0,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 1,
      nmo: '00'O,
      ura_Identity: '0000000000000010'B,
      t3212: '1E'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NotConfigured,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 2000,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }
    )

TTCN Test Step: ts_CountConfiguredCell::lt_CheckOneCell

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10837
          }
        ]
      },
      attenuationLevel: 30,
      priScrmCode: 250,
      powerpCPICH: -55,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 321,
      sfnOffset: 3000,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 1,
      nmo: '00'O,
      ura_Identity: '0000000000000010'B,
      t3212: '1E'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NotConfigured,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 0,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }
    )

TTCN Test Step: ts_CountConfiguredCell::lt_CheckOneCell

(To search, click here and then press Ctrl+F)

    {
      cellId: 4,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10837
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 300,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 833,
      sfnOffset: 3000,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 1,
      nmo: '00'O,
      ura_Identity: '0000000000000011'B,
      t3212: '1E'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NotConfigured,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 4000,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }
    )

TTCN Test Step: ts_CountConfiguredCell::lt_CheckOneCell

(To search, click here and then press Ctrl+F)

    {
      cellId: 5,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10837
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 350,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 6577,
      sfnOffset: 678,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 1,
      nmo: '00'O,
      ura_Identity: '0000000000000011'B,
      t3212: '1E'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NotConfigured,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 5000,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }
    )

TTCN Test Step: ts_CountConfiguredCell::lt_CheckOneCell

(To search, click here and then press Ctrl+F)

    {
      cellId: 6,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 400,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 7253,
      sfnOffset: 1356,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 1,
      nmo: '00'O,
      ura_Identity: '0000000000000100'B,
      t3212: '1E'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NotConfigured,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 6000,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }
    )

TTCN Test Step: ts_CountConfiguredCell::lt_CheckOneCell

(To search, click here and then press Ctrl+F)

    {
      cellId: 7,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      attenuationLevel: 0,
      priScrmCode: 450,
      powerpCPICH: -60,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 4351,
      sfnOffset: 2034,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 1,
      nmo: '00'O,
      ura_Identity: '0000000000000100'B,
      t3212: '1E'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_NotConfigured,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 7000,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }
    )

TTCN Test Step: ts_InitializeSIB2AndSIB18

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10837
          }
        ]
      },
      attenuationLevel: 30,
      priScrmCode: 250,
      powerpCPICH: -55,
      powerpSCH: -5,
      powersSCH: -5,
      powerpCCPCH: -2,
      powersCCPCH: -2,
      powersCCPCH1: -2,
      timingsCCPCH1: 0,
      powerAICH: -5,
      powerPICH: -5,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      tCell: 321,
      sfnOffset: 3000,
      puncLimit: pl1,
      sf_PRACH: sfpr64,
      slotFormatsCCPCH1: 8,
      mcc: '001'H,
      mnc: '01F'H,
      lac: '0001'O,
      rac: '05'O,
      attFlag: 1,
      nmo: '00'O,
      ura_Identity: '0000000000000010'B,
      t3212: '1E'O,
      cRNTI: '0000000000000001'B,
      uRNTI:
      {
        srnc_Identity: '000000000001'B,
        s_RNTI: '00000000000000000001'B
      },
      cellConfig: cell_FACH_NoDedicated,
      dRX_CycleLength:
      {
        cN_CS_DRX_CycleLength: 7,
        cN_PS_DRX_CycleLength: 7,
        uTRAN_DRX_CycleLength: 9
      },
      uL_ScramblingCode: 0,
      DL_DPCH_SHO: GcFALSE,
      UL_DPCH_SHO: GcFALSE,
      dl_DPCH_2ndScrCode: 1
    }
    )

TTCN Test Step: ts_SendSIB1_LongNeighCellInfo

(To search, click here and then press Ctrl+F)

    {
      cn_CommonGSM_MAP_NAS_SysInfo: '0001'O,
      cn_DomainSysInfoList:
      [
        {
          cn_DomainIdentity: ps_domain,
          cn_Type:
          [
            gsm_MAP: '0500'O
          ],
          cn_DRX_CycleLengthCoeff: 7
        },

        {
          cn_DomainIdentity: cs_domain,
          cn_Type:
          [
            gsm_MAP: '1E01'O
          ],
          cn_DRX_CycleLengthCoeff: 7
        }
      ],
      ue_ConnTimersAndConstants:
      {
        t_301: OMIT,
        n_301: OMIT,
        t_302: OMIT,
        n_302: OMIT,
        t_304: OMIT,
        n_304: OMIT,
        t_305: OMIT,
        t_307: OMIT,
        t_308: OMIT,
        t_309: OMIT,
        t_310: OMIT,
        n_310: OMIT,
        t_311: OMIT,
        t_312: OMIT,
        n_312: OMIT,
        t_313: OMIT,
        n_313: OMIT,
        t_314: OMIT,
        t_315: OMIT,
        n_315: OMIT,
        t_316: OMIT,
        t_317: OMIT
      },
      ue_IdleTimersAndConstants:
      {
        t_300: ms4000,
        n_300: 3,
        t_312: 10,
        n_312: s1
      },
      v3a0NonCriticalExtensions: OMIT
    }
    )

TTCN Test Step: ts_SendSIB2_LongNeighCellInfo

(To search, click here and then press Ctrl+F)

    {
      ura_IdentityList:
      [
        '0000000000000010'B
      ],
      nonCriticalExtensions: OMIT
    }
    )

TTCN Test Step: ts_SendSIB3_LongNeighCellInfo

(To search, click here and then press Ctrl+F)

    {
      sib4indicator: GcTRUE,
      cellIdentity: '0000000000000000000000000011'B,
      cellSelectReselectInfo:
      {
        mappingInfo: OMIT,
        cellSelectQualityMeasure:
        [
          cpich_RSCP: NULL
        ],
        modeSpecificInfo:
        [
          fdd:
          {
            s_Intrasearch: 8,
            s_Intersearch: 8,
            s_SearchHCS: OMIT,
            rat_List:
            [
              {
                rat_Identifier: gsm,
                s_SearchRAT: -16,
                s_HCS_RAT: OMIT,
                s_Limit_SearchRAT: 0
              }
            ],
            q_QualMin: -24,
            q_RxlevMin: -40
          }
        ],
        q_Hyst_l_S: 2,
        t_Reselection_S: 0,
        hcs_ServingCellInformation: OMIT,
        maxAllowedUL_TX_Power: 21
      },
      cellAccessRestriction:
      {
        cellBarred:
        [
          notBarred: NULL
        ],
        cellReservedForOperatorUse: notReserved,
        cellReservationExtension: notReserved,
        accessClassBarredList:
        [
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred,
          notBarred
        ]
      },
      nonCriticalExtensions: OMIT
    }
    )

TTCN Test Step: ts_SendSIB4_LongNeighCellInfo

(To search, click here and then press Ctrl+F)

    {
      cellIdentity: '0000000000000000000000000011'B,
      cellSelectReselectInfo:
      {
        mappingInfo: OMIT,
        cellSelectQualityMeasure:
        [
          cpich_RSCP: NULL
        ],
        modeSpecificInfo:
        [
          fdd:
          {
            s_Intrasearch: 8,
            s_Intersearch: 8,
            s_SearchHCS: OMIT,
            rat_List:
            [
              {
                rat_Identifier: gsm,
                s_SearchRAT: -16,
                s_HCS_RAT: OMIT,
                s_Limit_SearchRAT: 0
              }
            ],
            q_QualMin: -24,
            q_RxlevMin: -40
          }
        ],
        q_Hyst_l_S: 0,
        t_Reselection_S: 0,
        hcs_ServingCellInformation: OMIT,
        maxAllowedUL_TX_Power: 21
      },
      cellAccessRestriction:
      {
        cellBarred:
        [
          notBarred: NULL
        ],
        cellReservedForOperatorUse: notReserved,
        cellReservationExtension: notReserved,
        accessClassBarredList: OMIT
      },
      nonCriticalExtensions: OMIT
    }
    )

TTCN Test Step: ts_SendSIB5_LongNeighCellInfo

(To search, click here and then press Ctrl+F)

    {
      sib6indicator: GcTRUE,
      pich_PowerOffset: -5,
      modeSpecificInfo:
      [
        fdd:
        {
          aich_PowerOffset: -5
        }
      ],
      primaryCCPCH_Info: OMIT,
      prach_SystemInformationList:
      [
        {
          prach_RACH_Info:
          {
            modeSpecificInfo:
            [
              fdd:
              {
                availableSignatures: '0000000011111111'B,
                availableSF: sfpr64,
                preambleScramblingCodeWordNumber: 0,
                puncturingLimit: pl1,
                availableSubChannelNumbers: '111111111111'B
              }
            ]
          },
          transportChannelIdentity: 15,
          rach_TransportFormatSet:
          [
            commonTransChTFS:
            {
              tti:
              [
                tti20:
                [
                  {
                    rlc_Size:
                    [
                      fdd:
                      {
                        octetModeRLC_SizeInfoType2:
                        [
                          sizeType1: 15
                        ]
                      }
                    ],
                    numberOfTbSizeList:
                    [
                      [
                        one: NULL
                      ]
                    ],
                    logicalChannelList:
                    [
                      configured: NULL
                    ]
                  },

                  {
                    rlc_Size:
                    [
                      fdd:
                      {
                        octetModeRLC_SizeInfoType2:
                        [
                          sizeType2: 3
                        ]
                      }
                    ],
                    numberOfTbSizeList:
                    [
                      [
                        one: NULL
                      ]
                    ],
                    logicalChannelList:
                    [
                      configured: NULL
                    ]
                  }
                ]
              ],
              semistaticTF_Information:
              {
                channelCodingType:
                [
                  convolutional: half
                ],
                rateMatchingAttribute# 150 # crc_Size# crc16
              }
            }
          ]
          # rach_TFCS#
          [
            normalTFCI_Signalling#
            [
              complete#
              {
                ctfcSize#
                [
                  ctfc2Bit#
                  [
                    {
                      ctfc2# 0 # powerOffsetInformation#
                      {
                        gainFactorInformation#
                        [
                          computedGainFactors# 0
                        ]
                        # powerOffsetPp_m# 0
                      }
                    }
                    #
                    {
                      ctfc2# 1 # powerOffsetInformation#
                      {
                        gainFactorInformation#
                        [
                          signalledGainFactors#
                          {
                            modeSpecificInfo#
                            [
                              fdd#
                              {
                                gainFactorBetaC# 11
                              }
                            ]
                            # gainFactorBetaD# 15 # referenceTFC_ID# 0
                          }
                        ]
                        # powerOffsetPp_m# 0
                      }
                    }
                  ]
                ]
              }
            ]
          ]
          # prach_Partitioning#
          [
            fdd#
            [
              {
                accessServiceClass_FDD# OMIT
              }
              #
              {
                accessServiceClass_FDD#
                {
                  availableSignatureStartIndex# 0 # availableSignatureEndIndex# 7 # assignedSubChannelNumber# '1111'B
                }
              }
              #
              {
                accessServiceClass_FDD# OMIT
              }
              #
              {
                accessServiceClass_FDD#
                {
                  availableSignatureStartIndex# 0 # availableSignatureEndIndex# 7 # assignedSubChannelNumber# '1111'B
                }
              }
              #
              {
                accessServiceClass_FDD# OMIT
              }
              #
              {
                accessServiceClass_FDD#
                {
                  availableSignatureStartIndex# 0 # availableSignatureEndIndex# 7 # assignedSubChannelNumber# '1111'B
                }
              }
              #
              {
                accessServiceClass_FDD# OMIT
              }
              #
              {
                accessServiceClass_FDD#
                {
                  availableSignatureStartIndex# 0 # availableSignatureEndIndex# 7 # assignedSubChannelNumber# '1111'B
                }
              }
            ]
          ]
          # persistenceScalingFactorList#
          [
            psf0_9# psf0_9# psf0_9# psf0_9# psf0_9# psf0_9
          ]
          # ac_To_ASC_MappingTable#
          [
            6 # 5 # 4 # 3 # 2 # 1 # 0
          ]
          # modeSpecificInfo#
          [
            fdd#
            {
              primaryCPICH_TX_Power# 31 # constantValue# #10 # prach_PowerOffset#
              {
                powerRampStep# 3 # preambleRetransMax# 4
              }
              # rach_TransmissionParameters#
              {
                mmax# 2 # nb01Min# 3 # nb01Max# 10
              }
              # aich_Info#
              {
                channelisationCode256# 3 # sttd_Indicator# GcFALSE # aich_TransmissionTiming# e0
              }
            }
          ]
        }
      ]
      # sCCPCH_SystemInformationList#
      [
        {
          secondaryCCPCH_Info#
          {
            modeSpecificInfo#
            [
              fdd#
              {
                dummy1# mayBeUsed# dummy2# OMIT# secondaryScramblingCode# OMIT# sttd_Indicator# GcFALSE # sf_AndCodeNumber#
                [
                  sf64# 1
                ]
                # pilotSymbolExistence# GcFALSE # tfci_Existence# GcTRUE # positionFixedOrFlexible# flexible# timingOffset# 0
              }
            ]
          }
          # tfcs#
          [
            normalTFCI_Signalling#
            [
              complete#
              {
                ctfcSize#
                [
                  ctfc4Bit#
                  [
                    {
                      ctfc4# 0 # powerOffsetInformation# OMIT
                    }
                    #
                    {
                      ctfc4# 1 # powerOffsetInformation# OMIT
                    }
                    #
                    {
                      ctfc4# 2 # powerOffsetInformation# OMIT
                    }
                    #
                    {
                      ctfc4# 3 # powerOffsetInformation# OMIT
                    }
                    #
                    {
                      ctfc4# 4 # powerOffsetInformation# OMIT
                    }
                    #
                    {
                      ctfc4# 5 # powerOffsetInformation# OMIT
                    }
                    #
                    {
                      ctfc4# 6 # powerOffsetInformation# OMIT
                    }
                    #
                    {
                      ctfc4# 8 # powerOffsetInformation# OMIT
                    }
                  ]
                ]
              }
            ]
          ]
          # fach_PCH_InformationList#
          [
            {
              transportFormatSet#
              [
                commonTransChTFS#
                {
                  tti#
                  [
                    tti10#
                    [
                      {
                        rlc_Size#
                        [
                          fdd#
                          {
                            octetModeRLC_SizeInfoType2#
                            [
                              sizeType1# 24
                            ]
                          }
                        ]
                        # numberOfTbSizeList#
                        [
                          [
                            zero# NULL
                          ]
                          #
                          [
                            one# NULL
                          ]
                        ]
                        # logicalChannelList#
                        [
                          allSizes# NULL
                        ]
                      }
                    ]
                  ]
                  # semistaticTF_Information#
                  {
                    channelCodingType#
                    [
                      convolutional# half
                    ]
                    # rateMatchingAttribute# 230 # crc_Size# crc16
                  }
                }
              ]
              # transportChannelIdentity# 12 # ctch_Indicator# GcFALSE
            }
            #
            {
              transportFormatSet#
              [
                commonTransChTFS#
                {
                  tti#
                  [
                    tti10#
                    [
                      {
                        rlc_Size#
                        [
                          fdd#
                          {
                            octetModeRLC_SizeInfoType2#
                            [
                              sizeType1# 15
                            ]
                          }
                        ]
                        # numberOfTbSizeList#
                        [
                          [
                            zero# NULL
                          ]
                          #
                          [
                            one# NULL
                          ]
                          #
                          [
                            small# 2
                          ]
                        ]
                        # logicalChannelList#
                        [
                          allSizes# NULL
                        ]
                      }
                    ]
                  ]
                  # semistaticTF_Information#
                  {
                    channelCodingType#
                    [
                      convolutional# half
                    ]
                    # rateMatchingAttribute# 220 # crc_Size# crc16
                  }
                }
              ]
              # transportChannelIdentity# 13 # ctch_Indicator# GcFALSE
            }
            #
            {
              transportFormatSet#
              [
                commonTransChTFS#
                {
                  tti#
                  [
                    tti10#
                    [
                      {
                        rlc_Size#
                        [
                          fdd#
                          {
                            octetModeRLC_SizeInfoType2#
                            [
                              sizeType2# 3
                            ]
                          }
                        ]
                        # numberOfTbSizeList#
                        [
                          [
                            zero# NULL
                          ]
                          #
                          [
                            one# NULL
                          ]
                        ]
                        # logicalChannelList#
                        [
                          allSizes# NULL
                        ]
                      }
                    ]
                  ]
                  # semistaticTF_Information#
                  {
                    channelCodingType#
                    [
                      turbo# NULL
                    ]
                    # rateMatchingAttribute# 130 # crc_Size# crc16
                  }
                }
              ]
              # transportChannelIdentity# 14 # ctch_Indicator# GcFALSE
            }
          ]
          # pich_Info#
          [
            fdd#
            {
              channelisationCode256# 2 # pi_CountPerFrame# e18# sttd_Indicator# GcFALSE
            }
          ]
        }
      ]
      # cbs_DRX_Level1Information# OMIT# nonCriticalExtensions# OMIT
    }
    )

TTCN Test Step: ts_SendSIB6_LongNeighCellInfo

(To search, click here and then press Ctrl+F)

    {
      pich_PowerOffset: -5,
      modeSpecificInfo:
      [
        fdd:
        {
          aich_PowerOffset: -5,
          dummy: OMIT
        }
      ],
      primaryCCPCH_Info: OMIT,
      prach_SystemInformationList: OMIT,
      sCCPCH_SystemInformationList: OMIT,
      cbs_DRX_Level1Information: OMIT,
      nonCriticalExtensions: OMIT
    }
    )

TTCN Test Step: ts_SendSIB7_LongNeighCellInfo

(To search, click here and then press Ctrl+F)

    {
      modeSpecificInfo:
      [
        fdd:
        {
          ul_Interference: -100
        }
      ],
      prach_Information_SIB5_List:
      [
        2
      ],
      prach_Information_SIB6_List:
      [
        2
      ],
      expirationTimeFactor: OMIT,
      nonCriticalExtensions: OMIT
    }
    )

TTCN Test Step: ts_SendSIB7_LongNeighCellInfo::lt_CompleteSIB7OrLastSIB12_CompleteSIB7

(To search, click here and then press Ctrl+F)

    {
      modeSpecificInfo:
      [
        fdd:
        {
          ul_Interference: -100
        }
      ],
      prach_Information_SIB5_List:
      [
        2
      ],
      prach_Information_SIB6_List:
      [
        2
      ],
      expirationTimeFactor: OMIT,
      nonCriticalExtensions: OMIT
    }
    )

TTCN Test Step: ts_SendSIB7_LongNeighCellInfo::lt_ConcatWithSIB3

(To search, click here and then press Ctrl+F)

    {
      modeSpecificInfo:
      [
        fdd:
        {
          ul_Interference: -100
        }
      ],
      prach_Information_SIB5_List:
      [
        2
      ],
      prach_Information_SIB6_List:
      [
        2
      ],
      expirationTimeFactor: OMIT,
      nonCriticalExtensions: OMIT
    }
    )

TTCN Test Step: ts_SendSIB7_LongNeighCellInfo::lt_ConcatWithSIB18

(To search, click here and then press Ctrl+F)

    {
      modeSpecificInfo:
      [
        fdd:
        {
          ul_Interference: -100
        }
      ],
      prach_Information_SIB5_List:
      [
        2
      ],
      prach_Information_SIB6_List:
      [
        2
      ],
      expirationTimeFactor: OMIT,
      nonCriticalExtensions: OMIT
    }
    )

TTCN Test Step: ts_SendSIB7_LongNeighCellInfo::lt_ConcatWithSIB4

(To search, click here and then press Ctrl+F)

    {
      modeSpecificInfo:
      [
        fdd:
        {
          ul_Interference: -100
        }
      ],
      prach_Information_SIB5_List:
      [
        2
      ],
      prach_Information_SIB6_List:
      [
        2
      ],
      expirationTimeFactor: OMIT,
      nonCriticalExtensions: OMIT
    }
    )

TTCN Test Step: ts_SendSIB11_LongNeighCellInfo

(To search, click here and then press Ctrl+F)

    {
      sib12indicator: GcTRUE,
      fach_MeasurementOccasionInfo: OMIT,
      measurementControlSysInfo:
      {
        use_of_HCS:
        [
          hcs_not_used:
          {
            cellSelectQualityMeasure:
            [
              cpich_RSCP:
              {
                intraFreqMeasurementSysInfo:
                {
                  intraFreqMeasurementID: OMIT,
                  intraFreqCellInfoSI_List:
                  {
                    removedIntraFreqCellList: OMIT,
                    newIntraFreqCellList:
                    [
                      {
                        intraFreqCellID: 3,
                        cellInfo:
                        {
                          cellIndividualOffset: OMIT,
                          referenceTimeDifferenceToCell: OMIT,
                          modeSpecificInfo:
                          [
                            fdd:
                            {
                              primaryCPICH_Info:
                              {
                                primaryScramblingCode: 250
                              },
                              primaryCPICH_TX_Power: OMIT,
                              readSFN_Indicator: GcFALSE,
                              tx_DiversityIndicator: GcFALSE
                            }
                          ],
                          cellSelectionReselectionInfo: OMIT
                        }
                      },

                      {
                        intraFreqCellID: 4,
                        cellInfo:
                        {
                          cellIndividualOffset: OMIT,
                          referenceTimeDifferenceToCell: OMIT,
                          modeSpecificInfo:
                          [
                            fdd:
                            {
                              primaryCPICH_Info:
                              {
                                primaryScramblingCode: 300
                              },
                              primaryCPICH_TX_Power: OMIT,
                              readSFN_Indicator: GcTRUE,
                              tx_DiversityIndicator: GcFALSE
                            }
                          ],
                          cellSelectionReselectionInfo: OMIT
                        }
                      },

                      {
                        intraFreqCellID: 5,
                        cellInfo:
                        {
                          cellIndividualOffset: OMIT,
                          referenceTimeDifferenceToCell: OMIT,
                          modeSpecificInfo:
                          [
                            fdd:
                            {
                              primaryCPICH_Info:
                              {
                                primaryScramblingCode: 350
                              },
                              primaryCPICH_TX_Power: OMIT,
                              readSFN_Indicator: GcTRUE,
                              tx_DiversityIndicator: GcFALSE
                            }
                          ],
                          cellSelectionReselectionInfo: OMIT
                        }
                      }
                    ]
                  },
                  intraFreqMeasQuantity:
                  {
                    filterCoefficient: OMIT,
                    modeSpecificInfo:
                    [
                      fdd:
                      {
                        intraFreqMeasQuantity_FDD: cpich_RSCP
                      }
                    ]
                  },
                  intraFreqReportingQuantityForRACH: OMIT,
                  maxReportedCellsOnRACH: OMIT,
                  reportingInfoForCellDCH:
                  {
                    intraFreqReportingQuantity:
                    {
                      activeSetReportingQuantities:
                      {
                        dummy: noReport,
                        cellIdentity_reportingIndicator: GcTRUE,
                        cellSynchronisationInfoReportingIndicator: GcFALSE,
                        modeSpecificInfo:
                        [
                          fdd:
                          {
                            cpich_Ec_N0_reportingIndicator: GcFALSE,
                            cpich_RSCP_reportingIndicator: GcTRUE,
                            pathloss_reportingIndicator: GcFALSE
                          }
                        ]
                      },
                      monitoredSetReportingQuantities:
                      {
                        dummy: noReport,
                        cellIdentity_reportingIndicator: GcTRUE,
                        cellSynchronisationInfoReportingIndicator: GcTRUE,
                        modeSpecificInfo:
                        [
                          fdd:
                          {
                            cpich_Ec_N0_reportingIndicator: GcFALSE,
                            cpich_RSCP_reportingIndicator: GcTRUE,
                            pathloss_reportingIndicator: GcFALSE
                          }
                        ]
                      },
                      detectedSetReportingQuantities: OMIT
                    },
                    measurementReportingMode:
                    {
                      measurementReportTransferMode: acknowledgedModeRLC,
                      periodicalOrEventTrigger: eventTrigger
                    },
                    reportCriteria:
                    [
                      intraFreqReportingCriteria:
                      {
                        eventCriteriaList:
                        [
                          {
                            event:
                            [
                              e1a:
                              {
                                triggeringCondition: monitoredSetCellsOnly,
                                reportingRange: 5,
                                forbiddenAffectCellList: OMIT,
                                w: 1,
                                reportDeactivationThreshold: t2,
                                reportingAmount: ra4,
                                reportingInterval: ri4
                              }
                            ],
                            hysteresis: 0,
                            timeToTrigger: ttt640,
                            reportingCellStatus:
                            [
                              withinActiveAndOrMonitoredUsedFreq: e3
                            ]
                          },

                          {
                            event:
                            [
                              e1b:
                              {
                                triggeringCondition: activeSetCellsOnly,
                                reportingRange: 5,
                                forbiddenAffectCellList: OMIT,
                                w: 1
                              }
                            ],
                            hysteresis: 0,
                            timeToTrigger: ttt640,
                            reportingCellStatus:
                            [
                              withinActiveAndOrMonitoredUsedFreq: e3
                            ]
                          },

                          {
                            event:
                            [
                              e1c:
                              {
                                replacementActivationThreshold: t3,
                                reportingAmount: ra4,
                                reportingInterval: ri4
                              }
                            ],
                            hysteresis: 0,
                            timeToTrigger: ttt640,
                            reportingCellStatus:
                            [
                              withinActiveAndOrMonitoredUsedFreq: e3
                            ]
                          }
                        ]
                      }
                    ]
                  }
                },
                interFreqMeasurementSysInfo:
                {
                  interFreqCellInfoSI_List:
                  {
                    removedInterFreqCellList: OMIT,
                    newInterFreqCellList:
                    [
                      {
                        interFreqCellID: 0,
                        frequencyInfo:
                        {
                          modeSpecificInfo:
                          [
                            fdd:
                            {
                              uarfcn_UL: OMIT,
                              uarfcn_DL: 10700
                            }
                          ]
                        },
                        cellInfo:
                        {
                          cellIndividualOffset: OMIT,
                          referenceTimeDifferenceToCell: OMIT,
                          modeSpecificInfo:
                          [
                            fdd:
                            {
                              primaryCPICH_Info:
                              {
                                primaryScramblingCode: 100
                              },
                              primaryCPICH_TX_Power: OMIT,
                              readSFN_Indicator: GcFALSE,
                              tx_DiversityIndicator: GcFALSE
                            }
                          ],
                          cellSelectionReselectionInfo: OMIT
                        }
                      },

                      {
                        interFreqCellID: 1,
                        frequencyInfo: OMIT,
                        cellInfo:
                        {
                          cellIndividualOffset: OMIT,
                          referenceTimeDifferenceToCell: OMIT,
                          modeSpecificInfo:
                          [
                            fdd:
                            {
                              primaryCPICH_Info:
                              {
                                primaryScramblingCode: 150
                              },
                              primaryCPICH_TX_Power: OMIT,
                              readSFN_Indicator: GcFALSE,
                              tx_DiversityIndicator: GcFALSE
                            }
                          ],
                          cellSelectionReselectionInfo: OMIT
                        }
                      },

                      {
                        interFreqCellID: 2,
                        frequencyInfo: OMIT,
                        cellInfo:
                        {
                          cellIndividualOffset: OMIT,
                          referenceTimeDifferenceToCell: OMIT,
                          modeSpecificInfo:
                          [
                            fdd:
                            {
                              primaryCPICH_Info:
                              {
                                primaryScramblingCode: 200
                              },
                              primaryCPICH_TX_Power: OMIT,
                              readSFN_Indicator: GcFALSE,
                              tx_DiversityIndicator: GcFALSE
                            }
                          ],
                          cellSelectionReselectionInfo: OMIT
                        }
                      },

                      {
                        interFreqCellID: 6,
                        frequencyInfo: OMIT,
                        cellInfo:
                        {
                          cellIndividualOffset: OMIT,
                          referenceTimeDifferenceToCell: OMIT,
                          modeSpecificInfo:
                          [
                            fdd:
                            {
                              primaryCPICH_Info:
                              {
                                primaryScramblingCode: 400
                              },
                              primaryCPICH_TX_Power: OMIT,
                              readSFN_Indicator: GcFALSE,
                              tx_DiversityIndicator: GcFALSE
                            }
                          ],
                          cellSelectionReselectionInfo: OMIT
                        }
                      },

                      {
                        interFreqCellID: 7,
                        frequencyInfo: OMIT,
                        cellInfo:
                        {
                          cellIndividualOffset: OMIT,
                          referenceTimeDifferenceToCell: OMIT,
                          modeSpecificInfo:
                          [
                            fdd:
                            {
                              primaryCPICH_Info:
                              {
                                primaryScramblingCode: 450
                              },
                              primaryCPICH_TX_Power: OMIT,
                              readSFN_Indicator: GcFALSE,
                              tx_DiversityIndicator: GcFALSE
                            }
                          ],
                          cellSelectionReselectionInfo: OMIT
                        }
                      }
                    ]
                  }
                }
              }
            ],
            interRATMeasurementSysInfo: OMIT
          }
        ],
        trafficVolumeMeasSysInfo: OMIT,
        dummy: OMIT
      },
      nonCriticalExtensions: OMIT
    }
    )

TTCN Test Step: ts_SendSIB12_LongNeighCellInfo

(To search, click here and then press Ctrl+F)

    {
      fach_MeasurementOccasionInfo: OMIT,
      measurementControlSysInfo:
      {
        use_of_HCS:
        [
          hcs_not_used:
          {
            cellSelectQualityMeasure:
            [
              cpich_RSCP:
              {
                intraFreqMeasurementSysInfo: OMIT,
                interFreqMeasurementSysInfo: OMIT
              }
            ],
            interRATMeasurementSysInfo: OMIT
          }
        ],
        trafficVolumeMeasSysInfo: OMIT,
        dummy: OMIT
      },
      nonCriticalExtensions: OMIT
    }
    )

TTCN Test Step: ts_SendSIB12_LongNeighCellInfo::lt_CompleteSIB7

(To search, click here and then press Ctrl+F)

    {
      fach_MeasurementOccasionInfo: OMIT,
      measurementControlSysInfo:
      {
        use_of_HCS:
        [
          hcs_not_used:
          {
            cellSelectQualityMeasure:
            [
              cpich_RSCP:
              {
                intraFreqMeasurementSysInfo: OMIT,
                interFreqMeasurementSysInfo: OMIT
              }
            ],
            interRATMeasurementSysInfo: OMIT
          }
        ],
        trafficVolumeMeasSysInfo: OMIT,
        dummy: OMIT
      },
      nonCriticalExtensions: OMIT
    }
    )

TTCN Test Step: ts_SendSIB18_LongNeighCellInfo

(To search, click here and then press Ctrl+F)

    {
      idleModePLMNIdentities:
      {
        plmnsOfIntraFreqCellsList: OMIT,
        plmnsOfInterFreqCellsList: OMIT,
        plmnsOfInterRATCellsList: OMIT
      },
      connectedModePLMNIdentities: OMIT,
      nonCriticalExtensions: OMIT
    }
    )

TTCN Test Step: ts_SendSB1_LongNeighCellInfo

(To search, click here and then press Ctrl+F)

    {
      sib_ReferenceList:
      [
        {
          sib_Type:
          [
            sysInfoType6: 2
          ],
          scheduling:
          {
            scheduling:
            {
              segCount: OMIT,
              sib_Pos:
              [
                rep64: 2
              ],
              sib_PosOffsetInfo: OMIT
            }
          }
        },

        {
          sib_Type:
          [
            sysInfoType7: NULL
          ],
          scheduling:
          {
            scheduling:
            {
              segCount: OMIT,
              sib_Pos:
              [
                rep16: 7
              ],
              sib_PosOffsetInfo: OMIT
            }
          }
        },

        {
          sib_Type:
          [
            sysInfoType11: 2
          ],
          scheduling:
          {
            scheduling:
            {
              segCount: 2,
              sib_Pos:
              [
                rep64: 26
              ],
              sib_PosOffsetInfo:
              [
                so2
              ]
            }
          }
        },

        {
          sib_Type:
          [
            sysInfoType12: 2
          ],
          scheduling:
          {
            scheduling:
            {
              segCount: OMIT,
              sib_Pos:
              [
                rep64: 11
              ],
              sib_PosOffsetInfo: OMIT
            }
          }
        },

        {
          sib_Type:
          [
            sysInfoType18: 2
          ],
          scheduling:
          {
            scheduling:
            {
              segCount: OMIT,
              sib_Pos:
              [
                rep64: 23
              ],
              sib_PosOffsetInfo: OMIT
            }
          }
        }
      ],
      nonCriticalExtensions: OMIT
    }
    )

TTCN Test Step: ts_SendMIB

(To search, click here and then press Ctrl+F)

    {
      mib_ValueTag: 2,
      plmn_Type:
      [
        gsm_MAP:
        {
          plmn_Identity:
          {
            mcc:
            [
              0,
              0,
              1
            ],
            mnc:
            [
              0,
              1
            ]
          }
        }
      ],
      sibSb_ReferenceList:
      [
        {
          sibSb_Type:
          [
            sysInfoTypeSB1: 2
          ],
          scheduling:
          {
            scheduling:
            {
              segCount: OMIT,
              sib_Pos:
              [
                rep16: 1
              ],
              sib_PosOffsetInfo: OMIT
            }
          }
        },

        {
          sibSb_Type:
          [
            sysInfoType1: 2
          ],
          scheduling:
          {
            scheduling:
            {
              segCount: OMIT,
              sib_Pos:
              [
                rep64: 10
              ],
              sib_PosOffsetInfo: OMIT
            }
          }
        },

        {
          sibSb_Type:
          [
            sysInfoType2: 2
          ],
          scheduling:
          {
            scheduling:
            {
              segCount: OMIT,
              sib_Pos:
              [
                rep64: 10
              ],
              sib_PosOffsetInfo: OMIT
            }
          }
        },

        {
          sibSb_Type:
          [
            sysInfoType3: 2
          ],
          scheduling:
          {
            scheduling:
            {
              segCount: OMIT,
              sib_Pos:
              [
                rep64: 7
              ],
              sib_PosOffsetInfo: OMIT
            }
          }
        },

        {
          sibSb_Type:
          [
            sysInfoType4: 2
          ],
          scheduling:
          {
            scheduling:
            {
              segCount: OMIT,
              sib_Pos:
              [
                rep64: 31
              ],
              sib_PosOffsetInfo: OMIT
            }
          }
        },

        {
          sibSb_Type:
          [
            sysInfoType5: 2
          ],
          scheduling:
          {
            scheduling:
            {
              segCount: 3,
              sib_Pos:
              [
                rep64: 18
              ],
              sib_PosOffsetInfo:
              [
                so2,
                so4
              ]
            }
          }
        }
      ],
      nonCriticalExtensions: OMIT
    }
    )

TTCN Test Step: ts_CRLC_DL_Integrity

(To search, click here and then press Ctrl+F)

    {
      integrityProtectionModeCommand:
      [
        startIntegrityProtection:
        {
          integrityProtInitNumber: '00001111000011110000111100001111'B
        }
      ],
      integrityProtectionAlgorithm: uia1
    }
    )

TTCN Test Step: ts_CRLC_UL_CipherCfg

(To search, click here and then press Ctrl+F)

    [
      {
        rb_Identity: 1,
        rlc_SequenceNumber: 0
      },

      {
        rb_Identity: 2,
        rlc_SequenceNumber: 7
      },

      {
        rb_Identity: 3,
        rlc_SequenceNumber: 4
      },

      {
        rb_Identity: 4,
        rlc_SequenceNumber: 0
      }
    ]
    )

TTCN Test Step: ts_CRLC_DL_Integrity

(To search, click here and then press Ctrl+F)

    {
      integrityProtectionModeCommand:
      [
        startIntegrityProtection:
        {
          integrityProtInitNumber: '00001111000011110000111100001111'B
        }
      ],
      integrityProtectionAlgorithm: uia1
    }
    )

TTCN Test Step: ts_CRLC_UL_CipherCfg

(To search, click here and then press Ctrl+F)

    [
      {
        rb_Identity: 1,
        rlc_SequenceNumber: 0
      },

      {
        rb_Identity: 2,
        rlc_SequenceNumber: 7
      },

      {
        rb_Identity: 3,
        rlc_SequenceNumber: 5
      },

      {
        rb_Identity: 4,
        rlc_SequenceNumber: 0
      }
    ]
    )

TTCN Test Step: ts_CRLC_DL_Integrity

(To search, click here and then press Ctrl+F)

    {
      integrityProtectionModeCommand:
      [
        startIntegrityProtection:
        {
          integrityProtInitNumber: '00001111000011110000111100001111'B
        }
      ],
      integrityProtectionAlgorithm: uia1
    }
    )

TTCN Test Step: ts_CRLC_UL_CipherCfg

(To search, click here and then press Ctrl+F)

    [
      {
        rb_Identity: 1,
        rlc_SequenceNumber: 0
      },

      {
        rb_Identity: 2,
        rlc_SequenceNumber: 7
      },

      {
        rb_Identity: 3,
        rlc_SequenceNumber: 4
      },

      {
        rb_Identity: 4,
        rlc_SequenceNumber: 0
      }
    ]
    )

TTCN Test Step: ts_CMAC_DownloadSecurityKey

(To search, click here and then press Ctrl+F)

    '01000100011101110110011000010001000000000011001100100010110111011100110011111111111011101001100110001000101110111010101001010101'B  )

TTCN Test Step: ts_CMAC_DownloadSecurityKey

(To search, click here and then press Ctrl+F)

    '01000100011101110110011000010001000000000011001100100010110111011100110011111111111011101001100110001000101110111010101001010101'B  )