| RRC_wk26-tc_8_4_1_25ps_2004-07-12_13.09.01

TTCN PDU: CPHY_Cell_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      tcell: 0,
      sfnOffset: 0,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10700
          }
        ]
      },
      primaryScramblingCode_SS: 100,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      dLTxAttenuationLevel: 0
    }

TTCN PDU: CPHY_RL_Setup_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 0
      ],
      ratType: fdd,
      setupMessage:
      {
        physicalChannelInfo:
        [
          primaryCPICHInfo:
          {
            dl_TxPower_PCPICH: -60,
            txdiversityIndicator: GcFALSE
          }
        ]
      }
    }

TTCN PDU: CPHY_RL_Setup_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 1
      ],
      ratType: fdd,
      setupMessage:
      {
        physicalChannelInfo:
        [
          primarySCHInfo:
          {
            tstdIndicator: GcFALSE,
            dl_TxPower: -5
          }
        ]
      }
    }

TTCN PDU: CPHY_RL_Setup_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 2
      ],
      ratType: fdd,
      setupMessage:
      {
        physicalChannelInfo:
        [
          secondarySCHInfo:
          {
            tstdIndicator: GcFALSE,
            dl_TxPower: -5
          }
        ]
      }
    }

TTCN PDU: CPHY_RL_Setup_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 4
      ],
      ratType: fdd,
      setupMessage:
      {
        physicalChannelInfo:
        [
          primaryCCPCHInfo:
          {
            sttd_Indicator: GcFALSE,
            dl_TxPower: -2
          }
        ]
      }
    }

TTCN PDU: CPHY_TrCH_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 4
      ],
      ratType: fdd,
      trchConfigType:
      [
        nonDch: NULL
      ],
      configMessage:
      {
        activationTime:
        [
          activateNow: NULL
        ],
        ulconnectedTrCHList: OMIT,
        ulTFCS: OMIT,
        dlconnectedTrCHList:
        [
          {
            trchid: 11,
            dl_TransportChannelType: bch,
            transportChannelInfo:
            {
              tti:
              [
                tti20:
                [
                  {
                    tb_Size: 246,
                    numberOfTbSizeList:
                    [
                      [
                        one: NULL
                      ]
                    ],
                    logicalChannelList:
                    [
                      configured: NULL
                    ]
                  }
                ]
              ],
              semistaticTF_Information:
              {
                channelCodingType:
                [
                  convolutional: half
                ],
                rateMatchingAttribute# 1 # crc_Size# crc16
              }
            }
          }
        ]
        # dlTFCS#
        [
          normalTFCI_Signalling#
          [
            complete#
            {
              ctfcSize#
              [
                ctfc2Bit#
                [
                  {
                    ctfc2# 0 # powerOffsetInformation#
                    {
                      gainFactorInformation#
                      [
                        signalledGainFactors#
                        {
                          modeSpecificInfo#
                          [
                            fdd#
                            {
                              gainFactorBetaC# 11
                            }
                          ]
                          # gainFactorBetaD# 15 # referenceTFC_ID# 0
                        }
                      ]
                      # powerOffsetPp_m# OMIT
                    }
                  }
                ]
              ]
            }
          ]
        ]
      }
    }

TTCN PDU: CPHY_TrCH_Config_CNF

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 4
      ]
    }

TTCN PDU: CMAC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 4
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          activationTime:
          [
            activateNow: NULL
          ],
          uE_Info:
          {
            u_RNTI: OMIT,
            c_RNTI: OMIT
          },
          trCHInfo:
          {
            ulconnectedTrCHList: OMIT,
            ulTFCS: OMIT,
            dlconnectedTrCHList:
            [
              {
                trchid: 11,
                transportChannelInfo:
                {
                  tti:
                  [
                    tti20:
                    [
                      {
                        tb_Size: 246,
                        numberOfTbSizeList:
                        [
                          [
                            one: NULL
                          ]
                        ],
                        logicalChannelList:
                        [
                          configured: NULL
                        ]
                      }
                    ]
                  ],
                  semistaticTF_Information:
                  {
                    channelCodingType:
                    [
                      convolutional: half
                    ],
                    rateMatchingAttribute# 1 # crc_Size# crc16
                  }
                }
              }
            ]
            # dlTFCS#
            [
              normalTFCI_Signalling#
              [
                complete#
                {
                  ctfcSize#
                  [
                    ctfc2Bit#
                    [
                      {
                        ctfc2# 0 # powerOffsetInformation#
                        {
                          gainFactorInformation#
                          [
                            signalledGainFactors#
                            {
                              modeSpecificInfo#
                              [
                                fdd#
                                {
                                  gainFactorBetaC# 11
                                }
                              ]
                              # gainFactorBetaD# 15 # referenceTFC_ID# 0
                            }
                          ]
                          # powerOffsetPp_m# OMIT
                        }
                      }
                    ]
                  ]
                }
              ]
            ]
          }
          # trCH_LogCHMapping#
          {
            ulconnectedTrCHList# OMIT# dlconnectedTrCHList#
            [
              {
                trchid# 11 # trCH_LogCHMappingList#
                [
                  {
                    logicalChannel_Mapping#
                    [
                      dl_LogicalChannelMapping#
                      {
                        macHeaderManipulation# normalMacHeader# dl_TransportChannelType# bch# logicalChannelIdentity# 1 # logicalChannelType# bCCH# rlc_SizeList#
                        [
                          configured# NULL
                        ]
                        # mac_LogicalChannelPriority# 1
                      }
                    ]
                    # rB_Identity# #1 # cn_DomainIdentity# OMIT
                  }
                ]
              }
            ]
          }
        }
      ]
    }

TTCN PDU: CPHY_RL_Setup_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 5
      ],
      ratType: fdd,
      setupMessage:
      {
        physicalChannelInfo:
        [
          secondaryCCPCHInfo:
          {
            scramblingCode: 0,
            dl_ChannelizationCode:
            [
              sf64: 1
            ],
            sCCPCHSlotFormat: 8,
            timingOffset: 0,
            positionFixedOrFlexible: flexible,
            sttd_Indicator: GcFALSE,
            dl_TxPower: -2,
            powerOffsetOfTFCI_PO1: 6,
            powerOffsetOfPILOT_PO3: 6
          }
        ]
      }
    }

TTCN PDU: CPHY_TrCH_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 5
      ],
      ratType: fdd,
      trchConfigType:
      [
        nonDch: NULL
      ],
      configMessage:
      {
        activationTime:
        [
          activateNow: NULL
        ],
        ulconnectedTrCHList: OMIT,
        ulTFCS: OMIT,
        dlconnectedTrCHList:
        [
          {
            trchid: 12,
            dl_TransportChannelType: pch,
            transportChannelInfo:
            {
              tti:
              [
                tti10:
                [
                  {
                    tb_Size: 240,
                    numberOfTbSizeList:
                    [
                      [
                        zero: NULL
                      ],

                      [
                        one: NULL
                      ]
                    ],
                    logicalChannelList:
                    [
                      allSizes: NULL
                    ]
                  }
                ]
              ],
              semistaticTF_Information:
              {
                channelCodingType:
                [
                  convolutional: half
                ],
                rateMatchingAttribute# 230 # crc_Size# crc16
              }
            }
          }
          #
          {
            trchid# 13 # dl_TransportChannelType# fach# transportChannelInfo#
            {
              tti#
              [
                tti10#
                [
                  {
                    tb_Size# 168 # numberOfTbSizeList#
                    [
                      [
                        zero# NULL
                      ]
                      #
                      [
                        one# NULL
                      ]
                      #
                      [
                        small# 2
                      ]
                    ]
                    # logicalChannelList#
                    [
                      allSizes# NULL
                    ]
                  }
                ]
              ]
              # semistaticTF_Information#
              {
                channelCodingType#
                [
                  convolutional# half
                ]
                # rateMatchingAttribute# 220 # crc_Size# crc16
              }
            }
          }
          #
          {
            trchid# 14 # dl_TransportChannelType# fach# transportChannelInfo#
            {
              tti#
              [
                tti10#
                [
                  {
                    tb_Size# 360 # numberOfTbSizeList#
                    [
                      [
                        zero# NULL
                      ]
                      #
                      [
                        one# NULL
                      ]
                    ]
                    # logicalChannelList#
                    [
                      allSizes# NULL
                    ]
                  }
                ]
              ]
              # semistaticTF_Information#
              {
                channelCodingType#
                [
                  turbo# NULL
                ]
                # rateMatchingAttribute# 130 # crc_Size# crc16
              }
            }
          }
        ]
        # dlTFCS#
        [
          normalTFCI_Signalling#
          [
            complete#
            {
              ctfcSize#
              [
                ctfc4Bit#
                [
                  {
                    ctfc4# 0 # powerOffsetInformation#
                    {
                      gainFactorInformation#
                      [
                        computedGainFactors# 0
                      ]
                      # powerOffsetPp_m# OMIT
                    }
                  }
                  #
                  {
                    ctfc4# 1 # powerOffsetInformation#
                    {
                      gainFactorInformation#
                      [
                        computedGainFactors# 0
                      ]
                      # powerOffsetPp_m# OMIT
                    }
                  }
                  #
                  {
                    ctfc4# 2 # powerOffsetInformation#
                    {
                      gainFactorInformation#
                      [
                        computedGainFactors# 0
                      ]
                      # powerOffsetPp_m# OMIT
                    }
                  }
                  #
                  {
                    ctfc4# 3 # powerOffsetInformation#
                    {
                      gainFactorInformation#
                      [
                        computedGainFactors# 0
                      ]
                      # powerOffsetPp_m# OMIT
                    }
                  }
                  #
                  {
                    ctfc4# 4 # powerOffsetInformation#
                    {
                      gainFactorInformation#
                      [
                        computedGainFactors# 0
                      ]
                      # powerOffsetPp_m# OMIT
                    }
                  }
                  #
                  {
                    ctfc4# 5 # powerOffsetInformation#
                    {
                      gainFactorInformation#
                      [
                        computedGainFactors# 0
                      ]
                      # powerOffsetPp_m# OMIT
                    }
                  }
                  #
                  {
                    ctfc4# 6 # powerOffsetInformation#
                    {
                      gainFactorInformation#
                      [
                        computedGainFactors# 0
                      ]
                      # powerOffsetPp_m# OMIT
                    }
                  }
                  #
                  {
                    ctfc4# 8 # powerOffsetInformation#
                    {
                      gainFactorInformation#
                      [
                        signalledGainFactors#
                        {
                          modeSpecificInfo#
                          [
                            fdd#
                            {
                              gainFactorBetaC# 11
                            }
                          ]
                          # gainFactorBetaD# 15 # referenceTFC_ID# 0
                        }
                      ]
                      # powerOffsetPp_m# OMIT
                    }
                  }
                ]
              ]
            }
          ]
        ]
      }
    }

TTCN PDU: CMAC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 5
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          activationTime:
          [
            activateNow: NULL
          ],
          uE_Info:
          {
            u_RNTI: OMIT,
            c_RNTI: OMIT
          },
          trCHInfo:
          {
            ulconnectedTrCHList: OMIT,
            ulTFCS: OMIT,
            dlconnectedTrCHList:
            [
              {
                trchid: 12,
                transportChannelInfo:
                {
                  tti:
                  [
                    tti10:
                    [
                      {
                        tb_Size: 240,
                        numberOfTbSizeList:
                        [
                          [
                            zero: NULL
                          ],

                          [
                            one: NULL
                          ]
                        ],
                        logicalChannelList:
                        [
                          allSizes: NULL
                        ]
                      }
                    ]
                  ],
                  semistaticTF_Information:
                  {
                    channelCodingType:
                    [
                      convolutional: half
                    ],
                    rateMatchingAttribute# 230 # crc_Size# crc16
                  }
                }
              }
              #
              {
                trchid# 13 # transportChannelInfo#
                {
                  tti#
                  [
                    tti10#
                    [
                      {
                        tb_Size# 168 # numberOfTbSizeList#
                        [
                          [
                            zero# NULL
                          ]
                          #
                          [
                            one# NULL
                          ]
                          #
                          [
                            small# 2
                          ]
                        ]
                        # logicalChannelList#
                        [
                          allSizes# NULL
                        ]
                      }
                    ]
                  ]
                  # semistaticTF_Information#
                  {
                    channelCodingType#
                    [
                      convolutional# half
                    ]
                    # rateMatchingAttribute# 220 # crc_Size# crc16
                  }
                }
              }
              #
              {
                trchid# 14 # transportChannelInfo#
                {
                  tti#
                  [
                    tti10#
                    [
                      {
                        tb_Size# 360 # numberOfTbSizeList#
                        [
                          [
                            zero# NULL
                          ]
                          #
                          [
                            one# NULL
                          ]
                        ]
                        # logicalChannelList#
                        [
                          allSizes# NULL
                        ]
                      }
                    ]
                  ]
                  # semistaticTF_Information#
                  {
                    channelCodingType#
                    [
                      turbo# NULL
                    ]
                    # rateMatchingAttribute# 130 # crc_Size# crc16
                  }
                }
              }
            ]
            # dlTFCS#
            [
              normalTFCI_Signalling#
              [
                complete#
                {
                  ctfcSize#
                  [
                    ctfc4Bit#
                    [
                      {
                        ctfc4# 0 # powerOffsetInformation#
                        {
                          gainFactorInformation#
                          [
                            computedGainFactors# 0
                          ]
                          # powerOffsetPp_m# OMIT
                        }
                      }
                      #
                      {
                        ctfc4# 1 # powerOffsetInformation#
                        {
                          gainFactorInformation#
                          [
                            computedGainFactors# 0
                          ]
                          # powerOffsetPp_m# OMIT
                        }
                      }
                      #
                      {
                        ctfc4# 2 # powerOffsetInformation#
                        {
                          gainFactorInformation#
                          [
                            computedGainFactors# 0
                          ]
                          # powerOffsetPp_m# OMIT
                        }
                      }
                      #
                      {
                        ctfc4# 3 # powerOffsetInformation#
                        {
                          gainFactorInformation#
                          [
                            computedGainFactors# 0
                          ]
                          # powerOffsetPp_m# OMIT
                        }
                      }
                      #
                      {
                        ctfc4# 4 # powerOffsetInformation#
                        {
                          gainFactorInformation#
                          [
                            computedGainFactors# 0
                          ]
                          # powerOffsetPp_m# OMIT
                        }
                      }
                      #
                      {
                        ctfc4# 5 # powerOffsetInformation#
                        {
                          gainFactorInformation#
                          [
                            computedGainFactors# 0
                          ]
                          # powerOffsetPp_m# OMIT
                        }
                      }
                      #
                      {
                        ctfc4# 6 # powerOffsetInformation#
                        {
                          gainFactorInformation#
                          [
                            computedGainFactors# 0
                          ]
                          # powerOffsetPp_m# OMIT
                        }
                      }
                      #
                      {
                        ctfc4# 8 # powerOffsetInformation#
                        {
                          gainFactorInformation#
                          [
                            signalledGainFactors#
                            {
                              modeSpecificInfo#
                              [
                                fdd#
                                {
                                  gainFactorBetaC# 11
                                }
                              ]
                              # gainFactorBetaD# 15 # referenceTFC_ID# 0
                            }
                          ]
                          # powerOffsetPp_m# OMIT
                        }
                      }
                    ]
                  ]
                }
              ]
            ]
          }
          # trCH_LogCHMapping#
          {
            ulconnectedTrCHList# OMIT# dlconnectedTrCHList#
            [
              {
                trchid# 12 # trCH_LogCHMappingList#
                [
                  {
                    logicalChannel_Mapping#
                    [
                      dl_LogicalChannelMapping#
                      {
                        macHeaderManipulation# normalMacHeader# dl_TransportChannelType# pch# logicalChannelIdentity# 1 # logicalChannelType# pCCH# rlc_SizeList#
                        [
                          configured# NULL
                        ]
                        # mac_LogicalChannelPriority# 1
                      }
                    ]
                    # rB_Identity# #2 # cn_DomainIdentity# OMIT
                  }
                ]
              }
              #
              {
                trchid# 13 # trCH_LogCHMappingList#
                [
                  {
                    logicalChannel_Mapping#
                    [
                      dl_LogicalChannelMapping#
                      {
                        macHeaderManipulation# normalMacHeader# dl_TransportChannelType# fach# logicalChannelIdentity# 5 # logicalChannelType# cCCH# rlc_SizeList#
                        [
                          configured# NULL
                        ]
                        # mac_LogicalChannelPriority# 1
                      }
                    ]
                    # rB_Identity# 0 # cn_DomainIdentity# OMIT
                  }
                ]
              }
            ]
          }
        }
      ]
    }

TTCN PDU: CPHY_RL_Setup_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 6
      ],
      ratType: fdd,
      setupMessage:
      {
        physicalChannelInfo:
        [
          pICHInfo:
          {
            pichinfo:
            [
              fdd:
              {
                channelisationCode256: 2,
                pi_CountPerFrame: e18,
                sttd_Indicator: GcFALSE
              }
            ],
            dl_TxPower: -5,
            sccpchId_associated: 5
          }
        ]
      }
    }

TTCN PDU: CPHY_RL_Setup_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 7
      ],
      ratType: fdd,
      setupMessage:
      {
        physicalChannelInfo:
        [
          aICHInfo:
          {
            aichinfo:
            {
              channelisationCode256: 3,
              sttd_Indicator: GcFALSE,
              aich_TransmissionTiming: e0
            },
            dl_TxPower: -5
          }
        ]
      }
    }

TTCN PDU: CPHY_RL_Setup_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 8
      ],
      ratType: fdd,
      setupMessage:
      {
        physicalChannelInfo:
        [
          pRACHInfo:
          {
            fdd_tdd:
            [
              fdd:
              {
                preambleSignature: '0000000011111111'B,
                spreadingFactorForDataPart: sfpr64,
                preambleScramblingCode: 0,
                puncturingLimit: pl1,
                accessSlot: '111111111111'B
              }
            ]
          }
        ]
      }
    }

TTCN PDU: CPHY_TrCH_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 8
      ],
      ratType: fdd,
      trchConfigType:
      [
        nonDch: NULL
      ],
      configMessage:
      {
        activationTime:
        [
          activateNow: NULL
        ],
        ulconnectedTrCHList:
        [
          {
            trchid: 15,
            ul_TransportChannelType: rach,
            transportChannelInfo:
            {
              tti:
              [
                tti20:
                [
                  {
                    tb_Size: 168,
                    numberOfTbSizeList:
                    [
                      [
                        one: NULL
                      ]
                    ],
                    logicalChannelList:
                    [
                      configured: NULL
                    ]
                  },

                  {
                    tb_Size: 360,
                    numberOfTbSizeList:
                    [
                      [
                        one: NULL
                      ]
                    ],
                    logicalChannelList:
                    [
                      configured: NULL
                    ]
                  }
                ]
              ],
              semistaticTF_Information:
              {
                channelCodingType:
                [
                  convolutional: half
                ],
                rateMatchingAttribute# 150 # crc_Size# crc16
              }
            }
          }
        ]
        # ulTFCS#
        [
          normalTFCI_Signalling#
          [
            complete#
            {
              ctfcSize#
              [
                ctfc2Bit#
                [
                  {
                    ctfc2# 0 # powerOffsetInformation# OMIT
                  }
                  #
                  {
                    ctfc2# 1 # powerOffsetInformation# OMIT
                  }
                ]
              ]
            }
          ]
        ]
        # dlconnectedTrCHList# OMIT# dlTFCS# OMIT
      }
    }

TTCN PDU: CMAC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 8
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          activationTime:
          [
            activateNow: NULL
          ],
          uE_Info:
          {
            u_RNTI: OMIT,
            c_RNTI: OMIT
          },
          trCHInfo:
          {
            ulconnectedTrCHList:
            [
              {
                trchid: 15,
                transportChannelInfo:
                {
                  tti:
                  [
                    tti20:
                    [
                      {
                        tb_Size: 168,
                        numberOfTbSizeList:
                        [
                          [
                            one: NULL
                          ]
                        ],
                        logicalChannelList:
                        [
                          configured: NULL
                        ]
                      },

                      {
                        tb_Size: 360,
                        numberOfTbSizeList:
                        [
                          [
                            one: NULL
                          ]
                        ],
                        logicalChannelList:
                        [
                          configured: NULL
                        ]
                      }
                    ]
                  ],
                  semistaticTF_Information:
                  {
                    channelCodingType:
                    [
                      convolutional: half
                    ],
                    rateMatchingAttribute# 150 # crc_Size# crc16
                  }
                }
              }
            ]
            # ulTFCS#
            [
              normalTFCI_Signalling#
              [
                complete#
                {
                  ctfcSize#
                  [
                    ctfc2Bit#
                    [
                      {
                        ctfc2# 0 # powerOffsetInformation# OMIT
                      }
                      #
                      {
                        ctfc2# 1 # powerOffsetInformation# OMIT
                      }
                    ]
                  ]
                }
              ]
            ]
            # dlconnectedTrCHList# OMIT# dlTFCS# OMIT
          }
          # trCH_LogCHMapping#
          {
            ulconnectedTrCHList#
            [
              {
                trchid# 15 # trCH_LogCHMappingList#
                [
                  {
                    logicalChannel_Mapping#
                    [
                      ul_LogicalChannelMapping#
                      {
                        macHeaderManipulation# normalMacHeader# ul_TransportChannelType# rach# logicalChannelIdentity# 5 # logicalChannelType# cCCH
                      }
                    ]
                    # rB_Identity# 0 # cn_DomainIdentity# OMIT
                  }
                ]
              }
            ]
            # dlconnectedTrCHList# OMIT
          }
        }
      ]
    }

TTCN PDU: CPHY_RL_Setup_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 26
      ],
      ratType: fdd,
      setupMessage:
      {
        physicalChannelInfo:
        [
          dPCHInfo:
          {
            ul_DPCHInfo: OMIT,
            dl_DPCHInfo:
            {
              dl_CommonInformation:
              {
                dl_DPCH_InfoCommon:
                {
                  cfnHandling:
                  [
                    initialise:
                    {
                      cfntargetsfnframeoffset: OMIT
                    }
                  ],
                  modeSpecificInfo:
                  [
                    fdd:
                    {
                      dl_DPCH_PowerControlInfo:
                      {
                        modeSpecificInfo:
                        [
                          fdd:
                          {
                            dpc_Mode: singleTPC
                          }
                        ]
                      },
                      powerOffsetPilot_pdpdch: 0,
                      dl_rate_matching_restriction: OMIT,
                      spreadingFactorAndPilot:
                      [
                        sfd128: pb4
                      ],
                      positionFixedOrFlexible: fixed,
                      tfci_Existence: GcFALSE
                    }
                  ]
                },
                modeSpecificInfo:
                [
                  fdd:
                  {
                    defaultDPCH_OffsetValue: 0,
                    dpch_CompressedModeInfo: OMIT,
                    tx_DiversityMode: noDiversity,
                    ssdt_Information: OMIT
                  }
                ]
              },
              dl_DPCH_InfoPerRL:
              [
                fdd:
                {
                  pCPICH_UsageForChannelEst: mayBeUsed,
                  dpch_FrameOffset: 0,
                  secondaryCPICH_Info: OMIT,
                  dl_ChannelisationCodeList:
                  [
                    {
                      secondaryScramblingCode: 1,
                      sf_AndCodeNumber:
                      [
                        sf128: 0
                      ],
                      scramblingCodeChange: OMIT
                    }
                  ],
                  tpc_CombinationIndex: 0,
                  ssdt_CellIdentity: OMIT,
                  closedLoopTimingAdjMode: OMIT
                }
              ],
              powerOffsetOfTFCI_PO1: 0,
              powerOffsetOfTPC_PO2: 0,
              powerOffsetOfPILOT_PO3: 0,
              dl_TxPower: -5,
              dl_TxPowerMax: 15,
              dl_TxPowerMin: -35
            }
          }
        ]
      }
    }

TTCN PDU: CPHY_TrCH_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 26
      ],
      ratType: fdd,
      trchConfigType:
      [
        dch: Normal
      ],
      configMessage:
      {
        activationTime:
        [
          activateNow: NULL
        ],
        ulconnectedTrCHList: OMIT,
        ulTFCS: OMIT,
        dlconnectedTrCHList:
        [
          {
            trchid: 10,
            dl_TransportChannelType: dch,
            transportChannelInfo:
            {
              tti:
              [
                tti10:
                [
                  {
                    tb_Size: 148,
                    numberOfTbSizeList:
                    [
                      [
                        zero: NULL
                      ],

                      [
                        one: NULL
                      ]
                    ],
                    logicalChannelList:
                    [
                      allSizes: NULL
                    ]
                  }
                ]
              ],
              semistaticTF_Information:
              {
                channelCodingType:
                [
                  convolutional: third
                ],
                rateMatchingAttribute# 192 # crc_Size# crc16
              }
            }
          }
        ]
        # dlTFCS#
        [
          normalTFCI_Signalling#
          [
            complete#
            {
              ctfcSize#
              [
                ctfc2Bit#
                [
                  {
                    ctfc2# 0 # powerOffsetInformation#
                    {
                      gainFactorInformation#
                      [
                        computedGainFactors# 0
                      ]
                      # powerOffsetPp_m# OMIT
                    }
                  }
                  #
                  {
                    ctfc2# 1 # powerOffsetInformation#
                    {
                      gainFactorInformation#
                      [
                        signalledGainFactors#
                        {
                          modeSpecificInfo#
                          [
                            fdd#
                            {
                              gainFactorBetaC# 11
                            }
                          ]
                          # gainFactorBetaD# 15 # referenceTFC_ID# 0
                        }
                      ]
                      # powerOffsetPp_m# OMIT
                    }
                  }
                ]
              ]
            }
          ]
        ]
      }
    }

TTCN PDU: CPHY_TrCH_Config_CNF

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 26
      ]
    }

TTCN PDU: CMAC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        physicalChannelIdentity: 26
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          activationTime:
          [
            activateNow: NULL
          ],
          uE_Info:
          {
            u_RNTI: OMIT,
            c_RNTI: OMIT
          },
          trCHInfo:
          {
            ulconnectedTrCHList: OMIT,
            ulTFCS: OMIT,
            dlconnectedTrCHList:
            [
              {
                trchid: 10,
                transportChannelInfo:
                {
                  tti:
                  [
                    tti10:
                    [
                      {
                        tb_Size: 148,
                        numberOfTbSizeList:
                        [
                          [
                            zero: NULL
                          ],

                          [
                            one: NULL
                          ]
                        ],
                        logicalChannelList:
                        [
                          allSizes: NULL
                        ]
                      }
                    ]
                  ],
                  semistaticTF_Information:
                  {
                    channelCodingType:
                    [
                      convolutional: third
                    ],
                    rateMatchingAttribute# 192 # crc_Size# crc16
                  }
                }
              }
            ]
            # dlTFCS#
            [
              normalTFCI_Signalling#
              [
                complete#
                {
                  ctfcSize#
                  [
                    ctfc2Bit#
                    [
                      {
                        ctfc2# 0 # powerOffsetInformation#
                        {
                          gainFactorInformation#
                          [
                            computedGainFactors# 0
                          ]
                          # powerOffsetPp_m# OMIT
                        }
                      }
                      #
                      {
                        ctfc2# 1 # powerOffsetInformation#
                        {
                          gainFactorInformation#
                          [
                            signalledGainFactors#
                            {
                              modeSpecificInfo#
                              [
                                fdd#
                                {
                                  gainFactorBetaC# 11
                                }
                              ]
                              # gainFactorBetaD# 15 # referenceTFC_ID# 0
                            }
                          ]
                          # powerOffsetPp_m# OMIT
                        }
                      }
                    ]
                  ]
                }
              ]
            ]
          }
          # trCH_LogCHMapping#
          {
            ulconnectedTrCHList# OMIT# dlconnectedTrCHList#
            [
              {
                trchid# 10 # trCH_LogCHMappingList#
                [
                  {
                    logicalChannel_Mapping#
                    [
                      dl_LogicalChannelMapping#
                      {
                        macHeaderManipulation# normalMacHeader# dl_TransportChannelType# dch# logicalChannelIdentity# 1 # logicalChannelType# dCCH# rlc_SizeList#
                        [
                          configured# NULL
                        ]
                        # mac_LogicalChannelPriority# 1
                      }
                    ]
                    # rB_Identity# 1 # cn_DomainIdentity# OMIT
                  }
                  #
                  {
                    logicalChannel_Mapping#
                    [
                      dl_LogicalChannelMapping#
                      {
                        macHeaderManipulation# normalMacHeader# dl_TransportChannelType# dch# logicalChannelIdentity# 2 # logicalChannelType# dCCH# rlc_SizeList#
                        [
                          configured# NULL
                        ]
                        # mac_LogicalChannelPriority# 2
                      }
                    ]
                    # rB_Identity# 2 # cn_DomainIdentity# OMIT
                  }
                  #
                  {
                    logicalChannel_Mapping#
                    [
                      dl_LogicalChannelMapping#
                      {
                        macHeaderManipulation# normalMacHeader# dl_TransportChannelType# dch# logicalChannelIdentity# 3 # logicalChannelType# dCCH# rlc_SizeList#
                        [
                          configured# NULL
                        ]
                        # mac_LogicalChannelPriority# 3
                      }
                    ]
                    # rB_Identity# 3 # cn_DomainIdentity# OMIT
                  }
                  #
                  {
                    logicalChannel_Mapping#
                    [
                      dl_LogicalChannelMapping#
                      {
                        macHeaderManipulation# normalMacHeader# dl_TransportChannelType# dch# logicalChannelIdentity# 4 # logicalChannelType# dCCH# rlc_SizeList#
                        [
                          configured# NULL
                        ]
                        # mac_LogicalChannelPriority# 4
                      }
                    ]
                    # rB_Identity# 4 # cn_DomainIdentity# OMIT
                  }
                ]
              }
            ]
          }
        }
      ]
    }

TTCN PDU: CPHY_RL_Setup_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 20
      ],
      ratType: fdd,
      setupMessage:
      {
        physicalChannelInfo:
        [
          dPCHInfo:
          {
            ul_DPCHInfo:
            {
              ul_DPCH_PowerControlInfo:
              [
                fdd:
                {
                  dpcch_PowerOffset: -40,
                  pc_Preamble: 1,
                  sRB_delay: 7,
                  powerControlAlgorithm:
                  [
                    algorithm1: 1
                  ]
                }
              ],
              modeSpecificInfo:
              [
                fdd:
                {
                  scramblingCodeType: longSC,
                  scramblingCode: 0,
                  numberOfDPDCH: OMIT,
                  spreadingFactor: sf64,
                  tfci_Existence: GcTRUE,
                  numberOfFBI_Bits: OMIT,
                  puncturingLimit: pl1
                }
              ]
            },
            dl_DPCHInfo: OMIT
          }
        ]
      }
    }

TTCN PDU: CPHY_TrCH_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 20
      ],
      ratType: fdd,
      trchConfigType:
      [
        dch: Normal
      ],
      configMessage:
      {
        activationTime:
        [
          activateNow: NULL
        ],
        ulconnectedTrCHList:
        [
          {
            trchid: 5,
            ul_TransportChannelType: dch,
            transportChannelInfo:
            {
              tti:
              [
                tti10:
                [
                  {
                    tb_Size: 148,
                    numberOfTbSizeList:
                    [
                      [
                        zero: NULL
                      ],

                      [
                        one: NULL
                      ]
                    ],
                    logicalChannelList:
                    [
                      allSizes: NULL
                    ]
                  }
                ]
              ],
              semistaticTF_Information:
              {
                channelCodingType:
                [
                  convolutional: third
                ],
                rateMatchingAttribute# 192 # crc_Size# crc16
              }
            }
          }
        ]
        # ulTFCS#
        [
          normalTFCI_Signalling#
          [
            complete#
            {
              ctfcSize#
              [
                ctfc2Bit#
                [
                  {
                    ctfc2# 0 # powerOffsetInformation# OMIT
                  }
                  #
                  {
                    ctfc2# 1 # powerOffsetInformation# OMIT
                  }
                ]
              ]
            }
          ]
        ]
        # dlconnectedTrCHList# OMIT# dlTFCS# OMIT
      }
    }

TTCN PDU: CPHY_TrCH_Config_CNF

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 20
      ]
    }

TTCN PDU: CMAC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        physicalChannelIdentity: 20
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          activationTime:
          [
            activateNow: NULL
          ],
          uE_Info:
          {
            u_RNTI: OMIT,
            c_RNTI: OMIT
          },
          trCHInfo:
          {
            ulconnectedTrCHList:
            [
              {
                trchid: 5,
                transportChannelInfo:
                {
                  tti:
                  [
                    tti10:
                    [
                      {
                        tb_Size: 148,
                        numberOfTbSizeList:
                        [
                          [
                            zero: NULL
                          ],

                          [
                            one: NULL
                          ]
                        ],
                        logicalChannelList:
                        [
                          allSizes: NULL
                        ]
                      }
                    ]
                  ],
                  semistaticTF_Information:
                  {
                    channelCodingType:
                    [
                      convolutional: third
                    ],
                    rateMatchingAttribute# 192 # crc_Size# crc16
                  }
                }
              }
            ]
            # ulTFCS#
            [
              normalTFCI_Signalling#
              [
                complete#
                {
                  ctfcSize#
                  [
                    ctfc2Bit#
                    [
                      {
                        ctfc2# 0 # powerOffsetInformation# OMIT
                      }
                      #
                      {
                        ctfc2# 1 # powerOffsetInformation# OMIT
                      }
                    ]
                  ]
                }
              ]
            ]
            # dlconnectedTrCHList# OMIT# dlTFCS# OMIT
          }
          # trCH_LogCHMapping#
          {
            ulconnectedTrCHList#
            [
              {
                trchid# 5 # trCH_LogCHMappingList#
                [
                  {
                    logicalChannel_Mapping#
                    [
                      ul_LogicalChannelMapping#
                      {
                        macHeaderManipulation# normalMacHeader# ul_TransportChannelType# dch# logicalChannelIdentity# 1 # logicalChannelType# dCCH
                      }
                    ]
                    # rB_Identity# 1 # cn_DomainIdentity# OMIT
                  }
                  #
                  {
                    logicalChannel_Mapping#
                    [
                      ul_LogicalChannelMapping#
                      {
                        macHeaderManipulation# normalMacHeader# ul_TransportChannelType# dch# logicalChannelIdentity# 2 # logicalChannelType# dCCH
                      }
                    ]
                    # rB_Identity# 2 # cn_DomainIdentity# OMIT
                  }
                  #
                  {
                    logicalChannel_Mapping#
                    [
                      ul_LogicalChannelMapping#
                      {
                        macHeaderManipulation# normalMacHeader# ul_TransportChannelType# dch# logicalChannelIdentity# 3 # logicalChannelType# dCCH
                      }
                    ]
                    # rB_Identity# 3 # cn_DomainIdentity# OMIT
                  }
                  #
                  {
                    logicalChannel_Mapping#
                    [
                      ul_LogicalChannelMapping#
                      {
                        macHeaderManipulation# normalMacHeader# ul_TransportChannelType# dch# logicalChannelIdentity# 4 # logicalChannelType# dCCH
                      }
                    ]
                    # rB_Identity# 4 # cn_DomainIdentity# OMIT
                  }
                ]
              }
            ]
            # dlconnectedTrCHList# OMIT
          }
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          sS_rlc_Info:
          {
            sS_ul_RLC_Mode: OMIT,
            sS_dl_RLC_Mode:
            {
              dl_PayloadSize: 246,
              dl_RLCModeInfo:
              [
                ul_TM_RLC_Mode:
                {
                  transmissionRLC_Discard: OMIT,
                  segmentationIndication: GcFALSE
                }
              ]
            }
          },
          rB_LogCH_Mapping:
          {
            uLlogicalChannelIdentity: OMIT,
            dLlogicalChannelIdentity: 1,
            logicalChannelType: OMIT,
            cn_DomainIdentity: OMIT
          }
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -2
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          sS_rlc_Info:
          {
            sS_ul_RLC_Mode: OMIT,
            sS_dl_RLC_Mode:
            {
              dl_PayloadSize: 240,
              dl_RLCModeInfo:
              [
                ul_TM_RLC_Mode:
                {
                  transmissionRLC_Discard: OMIT,
                  segmentationIndication: GcFALSE
                }
              ]
            }
          },
          rB_LogCH_Mapping:
          {
            uLlogicalChannelIdentity: OMIT,
            dLlogicalChannelIdentity: 1,
            logicalChannelType: OMIT,
            cn_DomainIdentity: OMIT
          }
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: 0
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          sS_rlc_Info:
          {
            sS_ul_RLC_Mode: OMIT,
            sS_dl_RLC_Mode:
            {
              dl_PayloadSize: 152,
              dl_RLCModeInfo:
              [
                ul_UM_RLC_Mode:
                {
                  transmissionRLC_Discard:
                  [
                    timerBasedNoExplicit: dt100
                  ]
                }
              ]
            }
          },
          rB_LogCH_Mapping:
          {
            uLlogicalChannelIdentity: OMIT,
            dLlogicalChannelIdentity: 5,
            logicalChannelType: OMIT,
            cn_DomainIdentity: OMIT
          }
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: 0
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          sS_rlc_Info:
          {
            sS_ul_RLC_Mode:
            [
              dl_TM_RLC_Mode:
              {
                segmentationIndication: GcFALSE
              }
            ],
            sS_dl_RLC_Mode:
            {
              dl_PayloadSize: 166,
              dl_RLCModeInfo:
              [
                ul_TM_RLC_Mode:
                {
                  transmissionRLC_Discard: OMIT,
                  segmentationIndication: GcFALSE
                }
              ]
            }
          },
          rB_LogCH_Mapping:
          {
            uLlogicalChannelIdentity: 5,
            dLlogicalChannelIdentity: OMIT,
            logicalChannelType: OMIT,
            cn_DomainIdentity: OMIT
          }
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 1
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          sS_rlc_Info:
          {
            sS_ul_RLC_Mode:
            [
              dl_UM_RLC_Mode: NULL
            ],
            sS_dl_RLC_Mode:
            {
              dl_PayloadSize: 136,
              dl_RLCModeInfo:
              [
                ul_UM_RLC_Mode:
                {
                  transmissionRLC_Discard:
                  [
                    timerBasedNoExplicit: dt100
                  ]
                }
              ]
            }
          },
          rB_LogCH_Mapping:
          {
            uLlogicalChannelIdentity: 1,
            dLlogicalChannelIdentity: 1,
            logicalChannelType: OMIT,
            cn_DomainIdentity: OMIT
          }
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 2
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          sS_rlc_Info:
          {
            sS_ul_RLC_Mode:
            [
              dl_AM_RLC_Mode:
              {
                inSequenceDelivery: GcTRUE,
                receivingWindowSize: rw32,
                dl_RLC_StatusInfo:
                {
                  timerStatusProhibit: tsp200,
                  timerEPC: OMIT,
                  missingPDU_Indicator: GcTRUE,
                  timerStatusPeriodic: OMIT
                }
              }
            ],
            sS_dl_RLC_Mode:
            {
              dl_PayloadSize: 128,
              dl_RLCModeInfo:
              [
                ul_AM_RLC_Mode:
                {
                  transmissionRLC_Discard:
                  [
                    noDiscard: dat15
                  ],
                  transmissionWindowSize: tw32,
                  timerRST: tr500,
                  max_RST: rst1,
                  pollingInfo:
                  {
                    timerPollProhibit: tpp200,
                    timerPoll: tp200,
                    poll_PDU: OMIT,
                    poll_SDU: sdu1,
                    lastTransmissionPDU_Poll: GcTRUE,
                    lastRetransmissionPDU_Poll: GcTRUE,
                    pollWindow: pw99,
                    timerPollPeriodic: OMIT
                  }
                }
              ]
            }
          },
          rB_LogCH_Mapping:
          {
            uLlogicalChannelIdentity: 2,
            dLlogicalChannelIdentity: 2,
            logicalChannelType: OMIT,
            cn_DomainIdentity: OMIT
          }
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 3
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          sS_rlc_Info:
          {
            sS_ul_RLC_Mode:
            [
              dl_AM_RLC_Mode:
              {
                inSequenceDelivery: GcTRUE,
                receivingWindowSize: rw32,
                dl_RLC_StatusInfo:
                {
                  timerStatusProhibit: tsp200,
                  timerEPC: OMIT,
                  missingPDU_Indicator: GcTRUE,
                  timerStatusPeriodic: OMIT
                }
              }
            ],
            sS_dl_RLC_Mode:
            {
              dl_PayloadSize: 128,
              dl_RLCModeInfo:
              [
                ul_AM_RLC_Mode:
                {
                  transmissionRLC_Discard:
                  [
                    noDiscard: dat15
                  ],
                  transmissionWindowSize: tw32,
                  timerRST: tr500,
                  max_RST: rst1,
                  pollingInfo:
                  {
                    timerPollProhibit: tpp200,
                    timerPoll: tp200,
                    poll_PDU: OMIT,
                    poll_SDU: sdu1,
                    lastTransmissionPDU_Poll: GcTRUE,
                    lastRetransmissionPDU_Poll: GcTRUE,
                    pollWindow: pw99,
                    timerPollPeriodic: OMIT
                  }
                }
              ]
            }
          },
          rB_LogCH_Mapping:
          {
            uLlogicalChannelIdentity: 3,
            dLlogicalChannelIdentity: 3,
            logicalChannelType: OMIT,
            cn_DomainIdentity: OMIT
          }
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 4
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          sS_rlc_Info:
          {
            sS_ul_RLC_Mode:
            [
              dl_AM_RLC_Mode:
              {
                inSequenceDelivery: GcTRUE,
                receivingWindowSize: rw32,
                dl_RLC_StatusInfo:
                {
                  timerStatusProhibit: tsp200,
                  timerEPC: OMIT,
                  missingPDU_Indicator: GcTRUE,
                  timerStatusPeriodic: OMIT
                }
              }
            ],
            sS_dl_RLC_Mode:
            {
              dl_PayloadSize: 128,
              dl_RLCModeInfo:
              [
                ul_AM_RLC_Mode:
                {
                  transmissionRLC_Discard:
                  [
                    noDiscard: dat15
                  ],
                  transmissionWindowSize: tw32,
                  timerRST: tr500,
                  max_RST: rst1,
                  pollingInfo:
                  {
                    timerPollProhibit: tpp200,
                    timerPoll: tp200,
                    poll_PDU: OMIT,
                    poll_SDU: sdu1,
                    lastTransmissionPDU_Poll: GcTRUE,
                    lastRetransmissionPDU_Poll: GcTRUE,
                    pollWindow: pw99,
                    timerPollPeriodic: OMIT
                  }
                }
              ]
            }
          },
          rB_LogCH_Mapping:
          {
            uLlogicalChannelIdentity: 4,
            dLlogicalChannelIdentity: 4,
            logicalChannelType: OMIT,
            cn_DomainIdentity: OMIT
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 10,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              completeSIB_List:
              [
                {
                  sib_Type: systemInformationBlockType1,
                  sib_Data_variable: '1100010000000000000001011000100000101000000000100001000111100000000101000000000000000000000011000111010000'B
                },

                {
                  sib_Type: systemInformationBlockType2,
                  sib_Data_variable: '00000000000000000001'B
                }
              ]
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 10,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              completeSIB_List:
              [
                {
                  sib_Type: systemInformationBlockType1,
                  sib_Data_variable: '1100010000000000000001011000100000101000000000100001000111100000000101000000000000000000000011000111010000'B
                },

                {
                  sib_Type: systemInformationBlockType2,
                  sib_Data_variable: '00000000000000000001'B
                }
              ]
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 7,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              completeSIB_List:
              [
                {
                  sib_Type: systemInformationBlockType7,
                  sib_Data_variable: '100000101000000010000001'B
                },

                {
                  sib_Type: systemInformationBlockType3,
                  sib_Data_variable: '0100000000000000000000000000000010110111000110000000000000010000000000100100001000000100011111111111111111111111'B
                }
              ]
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 31,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              completeSIB_List:
              [
                {
                  sib_Type: systemInformationBlockType7,
                  sib_Data_variable: '100000101000000010000001'B
                },

                {
                  sib_Type: systemInformationBlockType4,
                  sib_Data_variable: '00000000000000000000000000000001011011100011000000000000001000000000010010000000000010001110111'B
                }
              ]
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 22,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              noSegment: NULL
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 18,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              firstSegment:
              {
                sib_Type: systemInformationBlockType5,
                seg_Count: 3,
                sib_Data_fixed: '000101010100010000111110000000001111111101000011111111111111110111010010000100001111000000101001000011000000101010100101010110000000000000001100110001011011010101111110001010111010000011111110100000111111101000001111111010'B
              }
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 19,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              subsequentSegment:
              {
                sib_Type: systemInformationBlockType5,
                segmentIndex: 1,
                sib_Data_fixed: '000011111111010000000000000000001101011000110100010000111111010011100101000001100001000011001010000000110000001110000001000000010110000010000000111000000000100010000110010000101001100100001010000000000011000000010001000101'B
              }
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 21,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              lastSegmentShort:
              {
                sib_Type: systemInformationBlockType5,
                segmentIndex: 2,
                sib_Data_variable: '1100101011010110100000000000011110001000011000000001011011011011011000100000000001000011000010001001010000001011011010000000010000'B
              }
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 2,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              completeSIB_List:
              [
                {
                  sib_Type: systemInformationBlockType6,
                  sib_Data_variable: '0000001010010001'B
                }
              ]
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 3,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              noSegment: NULL
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 5,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              noSegment: NULL
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 6,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              noSegment: NULL
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 15,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              completeSIB_List:
              [
                {
                  sib_Type: systemInformationBlockType7,
                  sib_Data_variable: '100000101000000010000001'B
                }
              ]
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 7,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              completeSIB_List:
              [
                {
                  sib_Type: systemInformationBlockType7,
                  sib_Data_variable: '100000101000000010000001'B
                },

                {
                  sib_Type: systemInformationBlockType3,
                  sib_Data_variable: '0100000000000000000000000000000010110111000110000000000000010000000000100100001000000100011111111111111111111111'B
                }
              ]
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 23,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              completeSIB_List:
              [
                {
                  sib_Type: systemInformationBlockType7,
                  sib_Data_variable: '100000101000000010000001'B
                },

                {
                  sib_Type: systemInformationBlockType18,
                  sib_Data_variable: '100000'B
                }
              ]
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 31,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              completeSIB_List:
              [
                {
                  sib_Type: systemInformationBlockType7,
                  sib_Data_variable: '100000101000000010000001'B
                },

                {
                  sib_Type: systemInformationBlockType4,
                  sib_Data_variable: '00000000000000000000000000000001011011100011000000000000001000000000010010000000000010001110111'B
                }
              ]
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 30,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              noSegment: NULL
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 29,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              noSegment: NULL
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 26,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              firstSegment:
              {
                sib_Type: systemInformationBlockType11,
                seg_Count: 2,
                sib_Data_fixed: '001000001101100100010010000000001000110010000100001000010010010110101000100000100110010001010011000001011001000010100111000010111000010100001000100010001100100101010100000001001010000101001010100001100001001010001000001010'B
              }
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 27,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              lastSegmentShort:
              {
                sib_Type: systemInformationBlockType11,
                segmentIndex: 1,
                sib_Data_variable: '000100001100001001010010011010101000011000010010101000101100011001010100101010100001001111101000100010000001010010110000100010100001010101111000'B
              }
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 11,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              completeSIB_List:
              [
                {
                  sib_Type: systemInformationBlockType12,
                  sib_Data_variable: '000000000'B
                }
              ]
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 13,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              noSegment: NULL
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 14,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              noSegment: NULL
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 15,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              completeSIB_List:
              [
                {
                  sib_Type: systemInformationBlockType7,
                  sib_Data_variable: '100000101000000010000001'B
                }
              ]
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 23,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              completeSIB_List:
              [
                {
                  sib_Type: systemInformationBlockType7,
                  sib_Data_variable: '100000101000000010000001'B
                },

                {
                  sib_Type: systemInformationBlockType18,
                  sib_Data_variable: '100000'B
                }
              ]
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 4,
        sg_POS: 1,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              completeSIB_List:
              [
                {
                  sib_Type: schedulingBlock1,
                  sib_Data_variable: '00010000101010001000001000110000010111010100111000101001101000000000010110100010001011110010100010010111'B
                }
              ]
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 3,
        sg_POS: 0,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              completeSIB_List:
              [
                {
                  sib_Type: masterInformationBlock,
                  sib_Data_variable: '0000000000000000010000000010010110101010000100010000000000001000100010100000101000100010100001001000100001110001101000100111110010001110010010010010000100000001'B
                }
              ]
            ]
          }
        }
      ]
    }

TTCN PDU: CPHY_Cell_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      tcell: 321,
      sfnOffset: 3000,
      frequencyInfo:
      {
        modeSpecificInfo:
        [
          fdd:
          {
            uarfcn_UL: OMIT,
            uarfcn_DL: 10837
          }
        ]
      },
      primaryScramblingCode_SS: 250,
      cellTxPowerLevel:
      [
        defaultCellTxPowerLvl: NULL
      ],
      dLTxAttenuationLevel: 30
    }

TTCN PDU: CPHY_RL_Setup_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        physicalChannelIdentity: 0
      ],
      ratType: fdd,
      setupMessage:
      {
        physicalChannelInfo:
        [
          primaryCPICHInfo:
          {
            dl_TxPower_PCPICH: -55,
            txdiversityIndicator: GcFALSE
          }
        ]
      }
    }

TTCN PDU: CPHY_RL_Setup_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        physicalChannelIdentity: 1
      ],
      ratType: fdd,
      setupMessage:
      {
        physicalChannelInfo:
        [
          primarySCHInfo:
          {
            tstdIndicator: GcFALSE,
            dl_TxPower: -5
          }
        ]
      }
    }

TTCN PDU: CPHY_RL_Setup_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        physicalChannelIdentity: 2
      ],
      ratType: fdd,
      setupMessage:
      {
        physicalChannelInfo:
        [
          secondarySCHInfo:
          {
            tstdIndicator: GcFALSE,
            dl_TxPower: -5
          }
        ]
      }
    }

TTCN PDU: CPHY_RL_Setup_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        physicalChannelIdentity: 4
      ],
      ratType: fdd,
      setupMessage:
      {
        physicalChannelInfo:
        [
          primaryCCPCHInfo:
          {
            sttd_Indicator: GcFALSE,
            dl_TxPower: -2
          }
        ]
      }
    }

TTCN PDU: CPHY_TrCH_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        physicalChannelIdentity: 4
      ],
      ratType: fdd,
      trchConfigType:
      [
        nonDch: NULL
      ],
      configMessage:
      {
        activationTime:
        [
          activateNow: NULL
        ],
        ulconnectedTrCHList: OMIT,
        ulTFCS: OMIT,
        dlconnectedTrCHList:
        [
          {
            trchid: 11,
            dl_TransportChannelType: bch,
            transportChannelInfo:
            {
              tti:
              [
                tti20:
                [
                  {
                    tb_Size: 246,
                    numberOfTbSizeList:
                    [
                      [
                        one: NULL
                      ]
                    ],
                    logicalChannelList:
                    [
                      configured: NULL
                    ]
                  }
                ]
              ],
              semistaticTF_Information:
              {
                channelCodingType:
                [
                  convolutional: half
                ],
                rateMatchingAttribute# 1 # crc_Size# crc16
              }
            }
          }
        ]
        # dlTFCS#
        [
          normalTFCI_Signalling#
          [
            complete#
            {
              ctfcSize#
              [
                ctfc2Bit#
                [
                  {
                    ctfc2# 0 # powerOffsetInformation#
                    {
                      gainFactorInformation#
                      [
                        signalledGainFactors#
                        {
                          modeSpecificInfo#
                          [
                            fdd#
                            {
                              gainFactorBetaC# 11
                            }
                          ]
                          # gainFactorBetaD# 15 # referenceTFC_ID# 0
                        }
                      ]
                      # powerOffsetPp_m# OMIT
                    }
                  }
                ]
              ]
            }
          ]
        ]
      }
    }

TTCN PDU: CPHY_TrCH_Config_CNF

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        physicalChannelIdentity: 4
      ]
    }

TTCN PDU: CMAC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        physicalChannelIdentity: 4
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          activationTime:
          [
            activateNow: NULL
          ],
          uE_Info:
          {
            u_RNTI: OMIT,
            c_RNTI: OMIT
          },
          trCHInfo:
          {
            ulconnectedTrCHList: OMIT,
            ulTFCS: OMIT,
            dlconnectedTrCHList:
            [
              {
                trchid: 11,
                transportChannelInfo:
                {
                  tti:
                  [
                    tti20:
                    [
                      {
                        tb_Size: 246,
                        numberOfTbSizeList:
                        [
                          [
                            one: NULL
                          ]
                        ],
                        logicalChannelList:
                        [
                          configured: NULL
                        ]
                      }
                    ]
                  ],
                  semistaticTF_Information:
                  {
                    channelCodingType:
                    [
                      convolutional: half
                    ],
                    rateMatchingAttribute# 1 # crc_Size# crc16
                  }
                }
              }
            ]
            # dlTFCS#
            [
              normalTFCI_Signalling#
              [
                complete#
                {
                  ctfcSize#
                  [
                    ctfc2Bit#
                    [
                      {
                        ctfc2# 0 # powerOffsetInformation#
                        {
                          gainFactorInformation#
                          [
                            signalledGainFactors#
                            {
                              modeSpecificInfo#
                              [
                                fdd#
                                {
                                  gainFactorBetaC# 11
                                }
                              ]
                              # gainFactorBetaD# 15 # referenceTFC_ID# 0
                            }
                          ]
                          # powerOffsetPp_m# OMIT
                        }
                      }
                    ]
                  ]
                }
              ]
            ]
          }
          # trCH_LogCHMapping#
          {
            ulconnectedTrCHList# OMIT# dlconnectedTrCHList#
            [
              {
                trchid# 11 # trCH_LogCHMappingList#
                [
                  {
                    logicalChannel_Mapping#
                    [
                      dl_LogicalChannelMapping#
                      {
                        macHeaderManipulation# normalMacHeader# dl_TransportChannelType# bch# logicalChannelIdentity# 1 # logicalChannelType# bCCH# rlc_SizeList#
                        [
                          configured# NULL
                        ]
                        # mac_LogicalChannelPriority# 1
                      }
                    ]
                    # rB_Identity# #1 # cn_DomainIdentity# OMIT
                  }
                ]
              }
            ]
          }
        }
      ]
    }

TTCN PDU: CPHY_RL_Setup_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        physicalChannelIdentity: 5
      ],
      ratType: fdd,
      setupMessage:
      {
        physicalChannelInfo:
        [
          secondaryCCPCHInfo:
          {
            scramblingCode: 0,
            dl_ChannelizationCode:
            [
              sf64: 1
            ],
            sCCPCHSlotFormat: 8,
            timingOffset: 0,
            positionFixedOrFlexible: flexible,
            sttd_Indicator: GcFALSE,
            dl_TxPower: -2,
            powerOffsetOfTFCI_PO1: 6,
            powerOffsetOfPILOT_PO3: 6
          }
        ]
      }
    }

TTCN PDU: CPHY_TrCH_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        physicalChannelIdentity: 5
      ],
      ratType: fdd,
      trchConfigType:
      [
        nonDch: NULL
      ],
      configMessage:
      {
        activationTime:
        [
          activateNow: NULL
        ],
        ulconnectedTrCHList: OMIT,
        ulTFCS: OMIT,
        dlconnectedTrCHList:
        [
          {
            trchid: 12,
            dl_TransportChannelType: pch,
            transportChannelInfo:
            {
              tti:
              [
                tti10:
                [
                  {
                    tb_Size: 240,
                    numberOfTbSizeList:
                    [
                      [
                        zero: NULL
                      ],

                      [
                        one: NULL
                      ]
                    ],
                    logicalChannelList:
                    [
                      allSizes: NULL
                    ]
                  }
                ]
              ],
              semistaticTF_Information:
              {
                channelCodingType:
                [
                  convolutional: half
                ],
                rateMatchingAttribute# 230 # crc_Size# crc16
              }
            }
          }
          #
          {
            trchid# 13 # dl_TransportChannelType# fach# transportChannelInfo#
            {
              tti#
              [
                tti10#
                [
                  {
                    tb_Size# 168 # numberOfTbSizeList#
                    [
                      [
                        zero# NULL
                      ]
                      #
                      [
                        one# NULL
                      ]
                      #
                      [
                        small# 2
                      ]
                    ]
                    # logicalChannelList#
                    [
                      allSizes# NULL
                    ]
                  }
                ]
              ]
              # semistaticTF_Information#
              {
                channelCodingType#
                [
                  convolutional# half
                ]
                # rateMatchingAttribute# 220 # crc_Size# crc16
              }
            }
          }
          #
          {
            trchid# 14 # dl_TransportChannelType# fach# transportChannelInfo#
            {
              tti#
              [
                tti10#
                [
                  {
                    tb_Size# 360 # numberOfTbSizeList#
                    [
                      [
                        zero# NULL
                      ]
                      #
                      [
                        one# NULL
                      ]
                    ]
                    # logicalChannelList#
                    [
                      allSizes# NULL
                    ]
                  }
                ]
              ]
              # semistaticTF_Information#
              {
                channelCodingType#
                [
                  turbo# NULL
                ]
                # rateMatchingAttribute# 130 # crc_Size# crc16
              }
            }
          }
        ]
        # dlTFCS#
        [
          normalTFCI_Signalling#
          [
            complete#
            {
              ctfcSize#
              [
                ctfc4Bit#
                [
                  {
                    ctfc4# 0 # powerOffsetInformation#
                    {
                      gainFactorInformation#
                      [
                        computedGainFactors# 0
                      ]
                      # powerOffsetPp_m# OMIT
                    }
                  }
                  #
                  {
                    ctfc4# 1 # powerOffsetInformation#
                    {
                      gainFactorInformation#
                      [
                        computedGainFactors# 0
                      ]
                      # powerOffsetPp_m# OMIT
                    }
                  }
                  #
                  {
                    ctfc4# 2 # powerOffsetInformation#
                    {
                      gainFactorInformation#
                      [
                        computedGainFactors# 0
                      ]
                      # powerOffsetPp_m# OMIT
                    }
                  }
                  #
                  {
                    ctfc4# 3 # powerOffsetInformation#
                    {
                      gainFactorInformation#
                      [
                        computedGainFactors# 0
                      ]
                      # powerOffsetPp_m# OMIT
                    }
                  }
                  #
                  {
                    ctfc4# 4 # powerOffsetInformation#
                    {
                      gainFactorInformation#
                      [
                        computedGainFactors# 0
                      ]
                      # powerOffsetPp_m# OMIT
                    }
                  }
                  #
                  {
                    ctfc4# 5 # powerOffsetInformation#
                    {
                      gainFactorInformation#
                      [
                        computedGainFactors# 0
                      ]
                      # powerOffsetPp_m# OMIT
                    }
                  }
                  #
                  {
                    ctfc4# 6 # powerOffsetInformation#
                    {
                      gainFactorInformation#
                      [
                        computedGainFactors# 0
                      ]
                      # powerOffsetPp_m# OMIT
                    }
                  }
                  #
                  {
                    ctfc4# 8 # powerOffsetInformation#
                    {
                      gainFactorInformation#
                      [
                        signalledGainFactors#
                        {
                          modeSpecificInfo#
                          [
                            fdd#
                            {
                              gainFactorBetaC# 11
                            }
                          ]
                          # gainFactorBetaD# 15 # referenceTFC_ID# 0
                        }
                      ]
                      # powerOffsetPp_m# OMIT
                    }
                  }
                ]
              ]
            }
          ]
        ]
      }
    }

TTCN PDU: CMAC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        physicalChannelIdentity: 5
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          activationTime:
          [
            activateNow: NULL
          ],
          uE_Info:
          {
            u_RNTI: OMIT,
            c_RNTI: OMIT
          },
          trCHInfo:
          {
            ulconnectedTrCHList: OMIT,
            ulTFCS: OMIT,
            dlconnectedTrCHList:
            [
              {
                trchid: 12,
                transportChannelInfo:
                {
                  tti:
                  [
                    tti10:
                    [
                      {
                        tb_Size: 240,
                        numberOfTbSizeList:
                        [
                          [
                            zero: NULL
                          ],

                          [
                            one: NULL
                          ]
                        ],
                        logicalChannelList:
                        [
                          allSizes: NULL
                        ]
                      }
                    ]
                  ],
                  semistaticTF_Information:
                  {
                    channelCodingType:
                    [
                      convolutional: half
                    ],
                    rateMatchingAttribute# 230 # crc_Size# crc16
                  }
                }
              }
              #
              {
                trchid# 13 # transportChannelInfo#
                {
                  tti#
                  [
                    tti10#
                    [
                      {
                        tb_Size# 168 # numberOfTbSizeList#
                        [
                          [
                            zero# NULL
                          ]
                          #
                          [
                            one# NULL
                          ]
                          #
                          [
                            small# 2
                          ]
                        ]
                        # logicalChannelList#
                        [
                          allSizes# NULL
                        ]
                      }
                    ]
                  ]
                  # semistaticTF_Information#
                  {
                    channelCodingType#
                    [
                      convolutional# half
                    ]
                    # rateMatchingAttribute# 220 # crc_Size# crc16
                  }
                }
              }
              #
              {
                trchid# 14 # transportChannelInfo#
                {
                  tti#
                  [
                    tti10#
                    [
                      {
                        tb_Size# 360 # numberOfTbSizeList#
                        [
                          [
                            zero# NULL
                          ]
                          #
                          [
                            one# NULL
                          ]
                        ]
                        # logicalChannelList#
                        [
                          allSizes# NULL
                        ]
                      }
                    ]
                  ]
                  # semistaticTF_Information#
                  {
                    channelCodingType#
                    [
                      turbo# NULL
                    ]
                    # rateMatchingAttribute# 130 # crc_Size# crc16
                  }
                }
              }
            ]
            # dlTFCS#
            [
              normalTFCI_Signalling#
              [
                complete#
                {
                  ctfcSize#
                  [
                    ctfc4Bit#
                    [
                      {
                        ctfc4# 0 # powerOffsetInformation#
                        {
                          gainFactorInformation#
                          [
                            computedGainFactors# 0
                          ]
                          # powerOffsetPp_m# OMIT
                        }
                      }
                      #
                      {
                        ctfc4# 1 # powerOffsetInformation#
                        {
                          gainFactorInformation#
                          [
                            computedGainFactors# 0
                          ]
                          # powerOffsetPp_m# OMIT
                        }
                      }
                      #
                      {
                        ctfc4# 2 # powerOffsetInformation#
                        {
                          gainFactorInformation#
                          [
                            computedGainFactors# 0
                          ]
                          # powerOffsetPp_m# OMIT
                        }
                      }
                      #
                      {
                        ctfc4# 3 # powerOffsetInformation#
                        {
                          gainFactorInformation#
                          [
                            computedGainFactors# 0
                          ]
                          # powerOffsetPp_m# OMIT
                        }
                      }
                      #
                      {
                        ctfc4# 4 # powerOffsetInformation#
                        {
                          gainFactorInformation#
                          [
                            computedGainFactors# 0
                          ]
                          # powerOffsetPp_m# OMIT
                        }
                      }
                      #
                      {
                        ctfc4# 5 # powerOffsetInformation#
                        {
                          gainFactorInformation#
                          [
                            computedGainFactors# 0
                          ]
                          # powerOffsetPp_m# OMIT
                        }
                      }
                      #
                      {
                        ctfc4# 6 # powerOffsetInformation#
                        {
                          gainFactorInformation#
                          [
                            computedGainFactors# 0
                          ]
                          # powerOffsetPp_m# OMIT
                        }
                      }
                      #
                      {
                        ctfc4# 8 # powerOffsetInformation#
                        {
                          gainFactorInformation#
                          [
                            signalledGainFactors#
                            {
                              modeSpecificInfo#
                              [
                                fdd#
                                {
                                  gainFactorBetaC# 11
                                }
                              ]
                              # gainFactorBetaD# 15 # referenceTFC_ID# 0
                            }
                          ]
                          # powerOffsetPp_m# OMIT
                        }
                      }
                    ]
                  ]
                }
              ]
            ]
          }
          # trCH_LogCHMapping#
          {
            ulconnectedTrCHList# OMIT# dlconnectedTrCHList#
            [
              {
                trchid# 12 # trCH_LogCHMappingList#
                [
                  {
                    logicalChannel_Mapping#
                    [
                      dl_LogicalChannelMapping#
                      {
                        macHeaderManipulation# normalMacHeader# dl_TransportChannelType# pch# logicalChannelIdentity# 1 # logicalChannelType# pCCH# rlc_SizeList#
                        [
                          configured# NULL
                        ]
                        # mac_LogicalChannelPriority# 1
                      }
                    ]
                    # rB_Identity# #2 # cn_DomainIdentity# OMIT
                  }
                ]
              }
              #
              {
                trchid# 13 # trCH_LogCHMappingList#
                [
                  {
                    logicalChannel_Mapping#
                    [
                      dl_LogicalChannelMapping#
                      {
                        macHeaderManipulation# normalMacHeader# dl_TransportChannelType# fach# logicalChannelIdentity# 5 # logicalChannelType# cCCH# rlc_SizeList#
                        [
                          configured# NULL
                        ]
                        # mac_LogicalChannelPriority# 1
                      }
                    ]
                    # rB_Identity# 0 # cn_DomainIdentity# OMIT
                  }
                ]
              }
            ]
          }
        }
      ]
    }

TTCN PDU: CPHY_RL_Setup_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        physicalChannelIdentity: 6
      ],
      ratType: fdd,
      setupMessage:
      {
        physicalChannelInfo:
        [
          pICHInfo:
          {
            pichinfo:
            [
              fdd:
              {
                channelisationCode256: 2,
                pi_CountPerFrame: e18,
                sttd_Indicator: GcFALSE
              }
            ],
            dl_TxPower: -5,
            sccpchId_associated: 5
          }
        ]
      }
    }

TTCN PDU: CPHY_RL_Setup_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        physicalChannelIdentity: 7
      ],
      ratType: fdd,
      setupMessage:
      {
        physicalChannelInfo:
        [
          aICHInfo:
          {
            aichinfo:
            {
              channelisationCode256: 3,
              sttd_Indicator: GcFALSE,
              aich_TransmissionTiming: e0
            },
            dl_TxPower: -5
          }
        ]
      }
    }

TTCN PDU: CPHY_RL_Setup_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        physicalChannelIdentity: 8
      ],
      ratType: fdd,
      setupMessage:
      {
        physicalChannelInfo:
        [
          pRACHInfo:
          {
            fdd_tdd:
            [
              fdd:
              {
                preambleSignature: '0000000011111111'B,
                spreadingFactorForDataPart: sfpr64,
                preambleScramblingCode: 0,
                puncturingLimit: pl1,
                accessSlot: '111111111111'B
              }
            ]
          }
        ]
      }
    }

TTCN PDU: CPHY_TrCH_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        physicalChannelIdentity: 8
      ],
      ratType: fdd,
      trchConfigType:
      [
        nonDch: NULL
      ],
      configMessage:
      {
        activationTime:
        [
          activateNow: NULL
        ],
        ulconnectedTrCHList:
        [
          {
            trchid: 15,
            ul_TransportChannelType: rach,
            transportChannelInfo:
            {
              tti:
              [
                tti20:
                [
                  {
                    tb_Size: 168,
                    numberOfTbSizeList:
                    [
                      [
                        one: NULL
                      ]
                    ],
                    logicalChannelList:
                    [
                      configured: NULL
                    ]
                  },

                  {
                    tb_Size: 360,
                    numberOfTbSizeList:
                    [
                      [
                        one: NULL
                      ]
                    ],
                    logicalChannelList:
                    [
                      configured: NULL
                    ]
                  }
                ]
              ],
              semistaticTF_Information:
              {
                channelCodingType:
                [
                  convolutional: half
                ],
                rateMatchingAttribute# 150 # crc_Size# crc16
              }
            }
          }
        ]
        # ulTFCS#
        [
          normalTFCI_Signalling#
          [
            complete#
            {
              ctfcSize#
              [
                ctfc2Bit#
                [
                  {
                    ctfc2# 0 # powerOffsetInformation# OMIT
                  }
                  #
                  {
                    ctfc2# 1 # powerOffsetInformation# OMIT
                  }
                ]
              ]
            }
          ]
        ]
        # dlconnectedTrCHList# OMIT# dlTFCS# OMIT
      }
    }

TTCN PDU: CMAC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        physicalChannelIdentity: 8
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          activationTime:
          [
            activateNow: NULL
          ],
          uE_Info:
          {
            u_RNTI: OMIT,
            c_RNTI: OMIT
          },
          trCHInfo:
          {
            ulconnectedTrCHList:
            [
              {
                trchid: 15,
                transportChannelInfo:
                {
                  tti:
                  [
                    tti20:
                    [
                      {
                        tb_Size: 168,
                        numberOfTbSizeList:
                        [
                          [
                            one: NULL
                          ]
                        ],
                        logicalChannelList:
                        [
                          configured: NULL
                        ]
                      },

                      {
                        tb_Size: 360,
                        numberOfTbSizeList:
                        [
                          [
                            one: NULL
                          ]
                        ],
                        logicalChannelList:
                        [
                          configured: NULL
                        ]
                      }
                    ]
                  ],
                  semistaticTF_Information:
                  {
                    channelCodingType:
                    [
                      convolutional: half
                    ],
                    rateMatchingAttribute# 150 # crc_Size# crc16
                  }
                }
              }
            ]
            # ulTFCS#
            [
              normalTFCI_Signalling#
              [
                complete#
                {
                  ctfcSize#
                  [
                    ctfc2Bit#
                    [
                      {
                        ctfc2# 0 # powerOffsetInformation# OMIT
                      }
                      #
                      {
                        ctfc2# 1 # powerOffsetInformation# OMIT
                      }
                    ]
                  ]
                }
              ]
            ]
            # dlconnectedTrCHList# OMIT# dlTFCS# OMIT
          }
          # trCH_LogCHMapping#
          {
            ulconnectedTrCHList#
            [
              {
                trchid# 15 # trCH_LogCHMappingList#
                [
                  {
                    logicalChannel_Mapping#
                    [
                      ul_LogicalChannelMapping#
                      {
                        macHeaderManipulation# normalMacHeader# ul_TransportChannelType# rach# logicalChannelIdentity# 5 # logicalChannelType# cCCH
                      }
                    ]
                    # rB_Identity# 0 # cn_DomainIdentity# OMIT
                  }
                ]
              }
            ]
            # dlconnectedTrCHList# OMIT
          }
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          sS_rlc_Info:
          {
            sS_ul_RLC_Mode: OMIT,
            sS_dl_RLC_Mode:
            {
              dl_PayloadSize: 246,
              dl_RLCModeInfo:
              [
                ul_TM_RLC_Mode:
                {
                  transmissionRLC_Discard: OMIT,
                  segmentationIndication: GcFALSE
                }
              ]
            }
          },
          rB_LogCH_Mapping:
          {
            uLlogicalChannelIdentity: OMIT,
            dLlogicalChannelIdentity: 1,
            logicalChannelType: OMIT,
            cn_DomainIdentity: OMIT
          }
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -2
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          sS_rlc_Info:
          {
            sS_ul_RLC_Mode: OMIT,
            sS_dl_RLC_Mode:
            {
              dl_PayloadSize: 240,
              dl_RLCModeInfo:
              [
                ul_TM_RLC_Mode:
                {
                  transmissionRLC_Discard: OMIT,
                  segmentationIndication: GcFALSE
                }
              ]
            }
          },
          rB_LogCH_Mapping:
          {
            uLlogicalChannelIdentity: OMIT,
            dLlogicalChannelIdentity: 1,
            logicalChannelType: OMIT,
            cn_DomainIdentity: OMIT
          }
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: 0
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          sS_rlc_Info:
          {
            sS_ul_RLC_Mode: OMIT,
            sS_dl_RLC_Mode:
            {
              dl_PayloadSize: 152,
              dl_RLCModeInfo:
              [
                ul_UM_RLC_Mode:
                {
                  transmissionRLC_Discard:
                  [
                    timerBasedNoExplicit: dt100
                  ]
                }
              ]
            }
          },
          rB_LogCH_Mapping:
          {
            uLlogicalChannelIdentity: OMIT,
            dLlogicalChannelIdentity: 5,
            logicalChannelType: OMIT,
            cn_DomainIdentity: OMIT
          }
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: 0
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          sS_rlc_Info:
          {
            sS_ul_RLC_Mode:
            [
              dl_TM_RLC_Mode:
              {
                segmentationIndication: GcFALSE
              }
            ],
            sS_dl_RLC_Mode:
            {
              dl_PayloadSize: 166,
              dl_RLCModeInfo:
              [
                ul_TM_RLC_Mode:
                {
                  transmissionRLC_Discard: OMIT,
                  segmentationIndication: GcFALSE
                }
              ]
            }
          },
          rB_LogCH_Mapping:
          {
            uLlogicalChannelIdentity: 5,
            dLlogicalChannelIdentity: OMIT,
            logicalChannelType: OMIT,
            cn_DomainIdentity: OMIT
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 10,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              completeSIB_List:
              [
                {
                  sib_Type: systemInformationBlockType1,
                  sib_Data_variable: '1100010000000000000001011000100000101000000000100001000111100000000101000000000000000000000011000111010000'B
                },

                {
                  sib_Type: systemInformationBlockType2,
                  sib_Data_variable: '00000000000000000010'B
                }
              ]
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 10,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              completeSIB_List:
              [
                {
                  sib_Type: systemInformationBlockType1,
                  sib_Data_variable: '1100010000000000000001011000100000101000000000100001000111100000000101000000000000000000000011000111010000'B
                },

                {
                  sib_Type: systemInformationBlockType2,
                  sib_Data_variable: '00000000000000000010'B
                }
              ]
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 7,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              completeSIB_List:
              [
                {
                  sib_Type: systemInformationBlockType7,
                  sib_Data_variable: '100000101000000010000001'B
                },

                {
                  sib_Type: systemInformationBlockType3,
                  sib_Data_variable: '0100000000000000000000000000110010110111000110000000000000010000000000100100001000000100011111111111111111111111'B
                }
              ]
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 31,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              completeSIB_List:
              [
                {
                  sib_Type: systemInformationBlockType7,
                  sib_Data_variable: '100000101000000010000001'B
                },

                {
                  sib_Type: systemInformationBlockType4,
                  sib_Data_variable: '00000000000000000000000000011001011011100011000000000000001000000000010010000000000010001110111'B
                }
              ]
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 22,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              noSegment: NULL
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 18,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              firstSegment:
              {
                sib_Type: systemInformationBlockType5,
                seg_Count: 3,
                sib_Data_fixed: '000101010100010000111110000000001111111101000011111111111111110111010010000100001111000000101001000011000000101010100101010110000000000000001100110001011011010101111110001010111010000011111110100000111111101000001111111010'B
              }
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 19,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              subsequentSegment:
              {
                sib_Type: systemInformationBlockType5,
                segmentIndex: 1,
                sib_Data_fixed: '000011111111010000000000000000001101011000110100010000111111010011100101000001100001000011001010000000110000001110000001000000010110000010000000111000000000100010000110010000101001100100001010000000000011000000010001000101'B
              }
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 21,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              lastSegmentShort:
              {
                sib_Type: systemInformationBlockType5,
                segmentIndex: 2,
                sib_Data_variable: '1100101011010110100000000000011110001000011000000001011011011011011000100000000001000011000010001001010000001011011010000000010000'B
              }
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 2,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              completeSIB_List:
              [
                {
                  sib_Type: systemInformationBlockType6,
                  sib_Data_variable: '0000001010010001'B
                }
              ]
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 3,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              noSegment: NULL
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 5,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              noSegment: NULL
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 6,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              noSegment: NULL
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 15,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              completeSIB_List:
              [
                {
                  sib_Type: systemInformationBlockType7,
                  sib_Data_variable: '100000101000000010000001'B
                }
              ]
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 7,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              completeSIB_List:
              [
                {
                  sib_Type: systemInformationBlockType7,
                  sib_Data_variable: '100000101000000010000001'B
                },

                {
                  sib_Type: systemInformationBlockType3,
                  sib_Data_variable: '0100000000000000000000000000110010110111000110000000000000010000000000100100001000000100011111111111111111111111'B
                }
              ]
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 23,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              completeSIB_List:
              [
                {
                  sib_Type: systemInformationBlockType7,
                  sib_Data_variable: '100000101000000010000001'B
                },

                {
                  sib_Type: systemInformationBlockType18,
                  sib_Data_variable: '100000'B
                }
              ]
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 31,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              completeSIB_List:
              [
                {
                  sib_Type: systemInformationBlockType7,
                  sib_Data_variable: '100000101000000010000001'B
                },

                {
                  sib_Type: systemInformationBlockType4,
                  sib_Data_variable: '00000000000000000000000000011001011011100011000000000000001000000000010010000000000010001110111'B
                }
              ]
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 30,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              noSegment: NULL
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 29,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              noSegment: NULL
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 26,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              firstSegment:
              {
                sib_Type: systemInformationBlockType11,
                seg_Count: 2,
                sib_Data_fixed: '001000001101100100001010001100001001111101000100100000010100101100101001010000101010111101000010001000100011001001010101000000010010100001010010101000011000010010100010000010100001000011000010010100100110101010000110000100'B
              }
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 27,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              lastSegmentShort:
              {
                sib_Type: systemInformationBlockType11,
                segmentIndex: 1,
                sib_Data_variable: '10101001001100000001010011100110000001000110010000100000100001001001011000100001000001001100100000100011000001011001000000100011100001011100001000'B
              }
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 11,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              completeSIB_List:
              [
                {
                  sib_Type: systemInformationBlockType12,
                  sib_Data_variable: '000000000'B
                }
              ]
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 13,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              noSegment: NULL
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 14,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              noSegment: NULL
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 15,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              completeSIB_List:
              [
                {
                  sib_Type: systemInformationBlockType7,
                  sib_Data_variable: '100000101000000010000001'B
                }
              ]
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 6,
        sg_POS: 23,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              completeSIB_List:
              [
                {
                  sib_Type: systemInformationBlockType7,
                  sib_Data_variable: '100000101000000010000001'B
                },

                {
                  sib_Type: systemInformationBlockType18,
                  sib_Data_variable: '100000'B
                }
              ]
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 4,
        sg_POS: 1,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              completeSIB_List:
              [
                {
                  sib_Type: schedulingBlock1,
                  sib_Data_variable: '00010000101010001000001000110000010111010100111000101001101000000000010110100010001011110010100010010111'B
                }
              ]
            ]
          }
        }
      ]
    }

TTCN PDU: CMAC_SYSINFO_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      {
        sg_REP: 3,
        sg_POS: 0,
        bcch_ModificationTime: OMIT
      }
    }

TTCN PDU: RLC_TR_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      tM_message:
      [
        bCCH_BCH_Message: PDU:
        {
          message:
          {
            sfn_Prime: 0,
            payload:
            [
              completeSIB_List:
              [
                {
                  sib_Type: masterInformationBlock,
                  sib_Data_variable: '0001000000000000010000000010010110101010000100010000000000001000100010100000101000100010100001001000100001110001101000100111110010001110010010010010000100000001'B
                }
              ]
            ]
          }
        }
      ]
    }

TTCN PDU: RLC_TR_DATA_IND

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: 0
      ],
      tM_message:
      [
        uL_CCCH_Message: PDU:
        {
          integrityCheckInfo: OMIT,
          message:
          [
            rrcConnectionRequest:
            {
              initialUE_Identity:
              [
                tmsi_and_LAI:
                {
                  tmsi: '00010001001000100011001101000100'B,
                  lai:
                  {
                    plmn_Identity:
                    {
                      mcc:
                      [
                        0,
                        0,
                        1
                      ],
                      mnc:
                      [
                        0,
                        1
                      ]
                    },
                    lac: '0000000000000001'B
                  }
                }
              ],
              establishmentCause: registration,
              protocolErrorIndicator: noError,
              measuredResultsOnRACH: OMIT,
              v3d0NonCriticalExtensions: OMIT
            }
          ]
        }
      ]
    }

TTCN PDU: RLC_UM_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: 0
      ],
      uM_message:
      [
        dL_CCCH_Message: PDU:
        {
          integrityCheckInfo: OMIT,
          message:
          [
            rrcConnectionSetup:
            [
              r3:
              {
                rrcConnectionSetup_r3:
                {
                  initialUE_Identity:
                  [
                    tmsi_and_LAI:
                    {
                      tmsi: '00010001001000100011001101000100'B,
                      lai:
                      {
                        plmn_Identity:
                        {
                          mcc:
                          [
                            0,
                            0,
                            1
                          ],
                          mnc:
                          [
                            0,
                            1
                          ]
                        },
                        lac: '0000000000000001'B
                      }
                    }
                  ],
                  rrc_TransactionIdentifier: 0,
                  activationTime: OMIT,
                  new_U_RNTI:
                  {
                    srnc_Identity: '000000000001'B,
                    s_RNTI: '00000000000000000001'B
                  },
                  new_c_RNTI: OMIT,
                  rrc_StateIndicator: cell_DCH,
                  utran_DRX_CycleLengthCoeff: 9,
                  capabilityUpdateRequirement:
                  {
                    ue_RadioCapabilityFDDUpdateRequirement: GcTRUE,
                    ue_RadioCapabilityTDDUpdateRequirement: GcFALSE,
                    systemSpecificCapUpdateReqList:
                    [
                      gsm
                    ]
                  },
                  srb_InformationSetupList:
                  [
                    {
                      rb_Identity: OMIT,
                      rlc_InfoChoice:
                      [
                        rlc_Info:
                        {
                          ul_RLC_Mode:
                          [
                            ul_UM_RLC_Mode:
                            {
                              transmissionRLC_Discard: OMIT
                            }
                          ],
                          dl_RLC_Mode:
                          [
                            dl_UM_RLC_Mode: NULL
                          ]
                        }
                      ],
                      rb_MappingInfo:
                      [
                        {
                          ul_LogicalChannelMappings:
                          [
                            oneLogicalChannel:
                            {
                              ul_TransportChannelType:
                              [
                                dch: 5
                              ],
                              logicalChannelIdentity: 1,
                              rlc_SizeList:
                              [
                                configured: NULL
                              ],
                              mac_LogicalChannelPriority: 1
                            }
                          ],
                          dl_LogicalChannelMappingList:
                          [
                            {
                              dl_TransportChannelType:
                              [
                                dch: 10
                              ],
                              logicalChannelIdentity: 1
                            }
                          ]
                        },

                        {
                          ul_LogicalChannelMappings:
                          [
                            oneLogicalChannel:
                            {
                              ul_TransportChannelType:
                              [
                                rach: NULL
                              ],
                              logicalChannelIdentity: 1,
                              rlc_SizeList:
                              [
                                explicitList:
                                [
                                  {
                                    rlc_SizeIndex: 1
                                  }
                                ]
                              ],
                              mac_LogicalChannelPriority: 1
                            }
                          ],
                          dl_LogicalChannelMappingList:
                          [
                            {
                              dl_TransportChannelType:
                              [
                                fach: NULL
                              ],
                              logicalChannelIdentity: 1
                            }
                          ]
                        }
                      ]
                    },

                    {
                      rb_Identity: OMIT,
                      rlc_InfoChoice:
                      [
                        rlc_Info:
                        {
                          ul_RLC_Mode:
                          [
                            ul_AM_RLC_Mode:
                            {
                              transmissionRLC_Discard:
                              [
                                noDiscard: dat15
                              ],
                              transmissionWindowSize: tw32,
                              timerRST: tr500,
                              max_RST: rst1,
                              pollingInfo:
                              {
                                timerPollProhibit: tpp200,
                                timerPoll: tp200,
                                poll_PDU: OMIT,
                                poll_SDU: sdu1,
                                lastTransmissionPDU_Poll: GcTRUE,
                                lastRetransmissionPDU_Poll: GcTRUE,
                                pollWindow: pw99,
                                timerPollPeriodic: OMIT
                              }
                            }
                          ],
                          dl_RLC_Mode:
                          [
                            dl_AM_RLC_Mode:
                            {
                              inSequenceDelivery: GcTRUE,
                              receivingWindowSize: rw32,
                              dl_RLC_StatusInfo:
                              {
                                timerStatusProhibit: tsp200,
                                timerEPC: OMIT,
                                missingPDU_Indicator: GcTRUE,
                                timerStatusPeriodic: OMIT
                              }
                            }
                          ]
                        }
                      ],
                      rb_MappingInfo:
                      [
                        {
                          ul_LogicalChannelMappings:
                          [
                            oneLogicalChannel:
                            {
                              ul_TransportChannelType:
                              [
                                dch: 5
                              ],
                              logicalChannelIdentity: 2,
                              rlc_SizeList:
                              [
                                configured: NULL
                              ],
                              mac_LogicalChannelPriority: 2
                            }
                          ],
                          dl_LogicalChannelMappingList:
                          [
                            {
                              dl_TransportChannelType:
                              [
                                dch: 10
                              ],
                              logicalChannelIdentity: 2
                            }
                          ]
                        },

                        {
                          ul_LogicalChannelMappings:
                          [
                            oneLogicalChannel:
                            {
                              ul_TransportChannelType:
                              [
                                rach: NULL
                              ],
                              logicalChannelIdentity: 2,
                              rlc_SizeList:
                              [
                                explicitList:
                                [
                                  {
                                    rlc_SizeIndex: 1
                                  }
                                ]
                              ],
                              mac_LogicalChannelPriority: 2
                            }
                          ],
                          dl_LogicalChannelMappingList:
                          [
                            {
                              dl_TransportChannelType:
                              [
                                fach: NULL
                              ],
                              logicalChannelIdentity: 2
                            }
                          ]
                        }
                      ]
                    },

                    {
                      rb_Identity: OMIT,
                      rlc_InfoChoice:
                      [
                        rlc_Info:
                        {
                          ul_RLC_Mode:
                          [
                            ul_AM_RLC_Mode:
                            {
                              transmissionRLC_Discard:
                              [
                                noDiscard: dat15
                              ],
                              transmissionWindowSize: tw32,
                              timerRST: tr500,
                              max_RST: rst1,
                              pollingInfo:
                              {
                                timerPollProhibit: tpp200,
                                timerPoll: tp200,
                                poll_PDU: OMIT,
                                poll_SDU: sdu1,
                                lastTransmissionPDU_Poll: GcTRUE,
                                lastRetransmissionPDU_Poll: GcTRUE,
                                pollWindow: pw99,
                                timerPollPeriodic: OMIT
                              }
                            }
                          ],
                          dl_RLC_Mode:
                          [
                            dl_AM_RLC_Mode:
                            {
                              inSequenceDelivery: GcTRUE,
                              receivingWindowSize: rw32,
                              dl_RLC_StatusInfo:
                              {
                                timerStatusProhibit: tsp200,
                                timerEPC: OMIT,
                                missingPDU_Indicator: GcTRUE,
                                timerStatusPeriodic: OMIT
                              }
                            }
                          ]
                        }
                      ],
                      rb_MappingInfo:
                      [
                        {
                          ul_LogicalChannelMappings:
                          [
                            oneLogicalChannel:
                            {
                              ul_TransportChannelType:
                              [
                                dch: 5
                              ],
                              logicalChannelIdentity: 3,
                              rlc_SizeList:
                              [
                                configured: NULL
                              ],
                              mac_LogicalChannelPriority: 3
                            }
                          ],
                          dl_LogicalChannelMappingList:
                          [
                            {
                              dl_TransportChannelType:
                              [
                                dch: 10
                              ],
                              logicalChannelIdentity: 3
                            }
                          ]
                        },

                        {
                          ul_LogicalChannelMappings:
                          [
                            oneLogicalChannel:
                            {
                              ul_TransportChannelType:
                              [
                                rach: NULL
                              ],
                              logicalChannelIdentity: 3,
                              rlc_SizeList:
                              [
                                explicitList:
                                [
                                  {
                                    rlc_SizeIndex: 1
                                  }
                                ]
                              ],
                              mac_LogicalChannelPriority: 3
                            }
                          ],
                          dl_LogicalChannelMappingList:
                          [
                            {
                              dl_TransportChannelType:
                              [
                                fach: NULL
                              ],
                              logicalChannelIdentity: 3
                            }
                          ]
                        }
                      ]
                    },

                    {
                      rb_Identity: OMIT,
                      rlc_InfoChoice:
                      [
                        rlc_Info:
                        {
                          ul_RLC_Mode:
                          [
                            ul_AM_RLC_Mode:
                            {
                              transmissionRLC_Discard:
                              [
                                noDiscard: dat15
                              ],
                              transmissionWindowSize: tw32,
                              timerRST: tr500,
                              max_RST: rst1,
                              pollingInfo:
                              {
                                timerPollProhibit: tpp200,
                                timerPoll: tp200,
                                poll_PDU: OMIT,
                                poll_SDU: sdu1,
                                lastTransmissionPDU_Poll: GcTRUE,
                                lastRetransmissionPDU_Poll: GcTRUE,
                                pollWindow: pw99,
                                timerPollPeriodic: OMIT
                              }
                            }
                          ],
                          dl_RLC_Mode:
                          [
                            dl_AM_RLC_Mode:
                            {
                              inSequenceDelivery: GcTRUE,
                              receivingWindowSize: rw32,
                              dl_RLC_StatusInfo:
                              {
                                timerStatusProhibit: tsp200,
                                timerEPC: OMIT,
                                missingPDU_Indicator: GcTRUE,
                                timerStatusPeriodic: OMIT
                              }
                            }
                          ]
                        }
                      ],
                      rb_MappingInfo:
                      [
                        {
                          ul_LogicalChannelMappings:
                          [
                            oneLogicalChannel:
                            {
                              ul_TransportChannelType:
                              [
                                dch: 5
                              ],
                              logicalChannelIdentity: 4,
                              rlc_SizeList:
                              [
                                configured: NULL
                              ],
                              mac_LogicalChannelPriority: 4
                            }
                          ],
                          dl_LogicalChannelMappingList:
                          [
                            {
                              dl_TransportChannelType:
                              [
                                dch: 10
                              ],
                              logicalChannelIdentity: 4
                            }
                          ]
                        },

                        {
                          ul_LogicalChannelMappings:
                          [
                            oneLogicalChannel:
                            {
                              ul_TransportChannelType:
                              [
                                rach: NULL
                              ],
                              logicalChannelIdentity: 4,
                              rlc_SizeList:
                              [
                                explicitList:
                                [
                                  {
                                    rlc_SizeIndex: 1
                                  }
                                ]
                              ],
                              mac_LogicalChannelPriority: 4
                            }
                          ],
                          dl_LogicalChannelMappingList:
                          [
                            {
                              dl_TransportChannelType:
                              [
                                fach: NULL
                              ],
                              logicalChannelIdentity: 4
                            }
                          ]
                        }
                      ]
                    }
                  ],
                  ul_CommonTransChInfo:
                  {
                    tfc_Subset: OMIT,
                    prach_TFCS: OMIT,
                    modeSpecificInfo:
                    [
                      fdd:
                      {
                        ul_TFCS:
                        [
                          normalTFCI_Signalling:
                          [
                            complete:
                            {
                              ctfcSize:
                              [
                                ctfc2Bit:
                                [
                                  {
                                    ctfc2: 0,
                                    powerOffsetInformation:
                                    {
                                      gainFactorInformation:
                                      [
                                        computedGainFactors: 0
                                      ],
                                      powerOffsetPp_m: OMIT
                                    }
                                  },

                                  {
                                    ctfc2: 1,
                                    powerOffsetInformation:
                                    {
                                      gainFactorInformation:
                                      [
                                        signalledGainFactors:
                                        {
                                          modeSpecificInfo:
                                          [
                                            fdd:
                                            {
                                              gainFactorBetaC: 11
                                            }
                                          ],
                                          gainFactorBetaD: 15,
                                          referenceTFC_ID: 0
                                        }
                                      ],
                                      powerOffsetPp_m: OMIT
                                    }
                                  }
                                ]
                              ]
                            }
                          ]
                        ]
                      }
                    ]
                  },
                  ul_AddReconfTransChInfoList:
                  [
                    {
                      ul_TransportChannelType: dch,
                      transportChannelIdentity: 5,
                      transportFormatSet:
                      [
                        dedicatedTransChTFS:
                        {
                          tti:
                          [
                            tti10:
                            [
                              {
                                rlc_Size:
                                [
                                  bitMode:
                                  [
                                    sizeType2:
                                    {
                                      part1: 2,
                                      part2: OMIT
                                    }
                                  ]
                                ],
                                numberOfTbSizeList:
                                [
                                  [
                                    zero: NULL
                                  ],

                                  [
                                    one: NULL
                                  ]
                                ],
                                logicalChannelList:
                                [
                                  allSizes: NULL
                                ]
                              }
                            ]
                          ],
                          semistaticTF_Information:
                          {
                            channelCodingType:
                            [
                              convolutional: third
                            ],
                            rateMatchingAttribute# 192 # crc_Size# crc16
                          }
                        }
                      ]
                    }
                  ]
                  # dl_CommonTransChInfo#
                  {
                    sccpch_TFCS# OMIT# modeSpecificInfo#
                    [
                      fdd#
                      {
                        dl_Parameters#
                        [
                          sameAsUL# NULL
                        ]
                      }
                    ]
                  }
                  # dl_AddReconfTransChInfoList#
                  [
                    {
                      dl_TransportChannelType# dch# dl_transportChannelIdentity# 10 # tfs_SignallingMode#
                      [
                        sameAsULTrCH#
                        {
                          ul_TransportChannelType# dch# ul_TransportChannelIdentity# 5
                        }
                      ]
                      # dch_QualityTarget#
                      {
                        bler_QualityValue# #20
                      }
                      # dummy# OMIT
                    }
                  ]
                  # frequencyInfo# OMIT# maxAllowedUL_TX_Power# OMIT# ul_ChannelRequirement#
                  [
                    ul_DPCH_Info#
                    {
                      ul_DPCH_PowerControlInfo#
                      [
                        fdd#
                        {
                          dpcch_PowerOffset# #40 # pc_Preamble# 1 # sRB_delay# 7 # powerControlAlgorithm#
                          [
                            algorithm1# 1
                          ]
                        }
                      ]
                      # modeSpecificInfo#
                      [
                        fdd#
                        {
                          scramblingCodeType# longSC# scramblingCode# 0 # numberOfDPDCH# OMIT# spreadingFactor# sf64# tfci_Existence# GcTRUE # numberOfFBI_Bits# OMIT# puncturingLimit# pl1
                        }
                      ]
                    }
                  ]
                  # dl_CommonInformation#
                  {
                    dl_DPCH_InfoCommon#
                    {
                      cfnHandling#
                      [
                        initialise#
                        {
                          cfntargetsfnframeoffset# OMIT
                        }
                      ]
                      # modeSpecificInfo#
                      [
                        fdd#
                        {
                          dl_DPCH_PowerControlInfo#
                          {
                            modeSpecificInfo#
                            [
                              fdd#
                              {
                                dpc_Mode# singleTPC
                              }
                            ]
                          }
                          # powerOffsetPilot_pdpdch# 0 # dl_rate_matching_restriction# OMIT# spreadingFactorAndPilot#
                          [
                            sfd128# pb4
                          ]
                          # positionFixedOrFlexible# fixed# tfci_Existence# GcFALSE
                        }
                      ]
                    }
                    # modeSpecificInfo#
                    [
                      fdd#
                      {
                        defaultDPCH_OffsetValue# 0 # dpch_CompressedModeInfo# OMIT# tx_DiversityMode# noDiversity# ssdt_Information# OMIT
                      }
                    ]
                  }
                  # dl_InformationPerRL_List#
                  [
                    {
                      modeSpecificInfo#
                      [
                        fdd#
                        {
                          primaryCPICH_Info#
                          {
                            primaryScramblingCode# 100
                          }
                          # pdsch_SHO_DCH_Info# OMIT# pdsch_CodeMapping# OMIT
                        }
                      ]
                      # dl_DPCH_InfoPerRL#
                      [
                        fdd#
                        {
                          pCPICH_UsageForChannelEst# mayBeUsed# dpch_FrameOffset# 0 # secondaryCPICH_Info# OMIT# dl_ChannelisationCodeList#
                          [
                            {
                              secondaryScramblingCode# 1 # sf_AndCodeNumber#
                              [
                                sf128# 0
                              ]
                              # scramblingCodeChange# noCodeChange
                            }
                          ]
                          # tpc_CombinationIndex# 0 # ssdt_CellIdentity# OMIT# closedLoopTimingAdjMode# OMIT
                        }
                      ]
                      # sccpch_InfoforFACH# OMIT
                    }
                  ]
                }
                # laterNonCriticalExtensions# OMIT
              }
            ]
          ]
        }
      ]
      # specialLI# GcTRUE
    }

TTCN PDU: RLC_AM_DATA_IND

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 2
      ],
      integrityResult:
      [
        integrityUsed: i_pass
      ],
      aM_message:
      [
        uL_DCCH_Message: PDU:
        {
          integrityCheckInfo: OMIT,
          message:
          [
            rrcConnectionSetupComplete:
            {
              rrc_TransactionIdentifier: 0,
              startList:
              [
                {
                  cn_DomainIdentity: ps_domain,
                  start_Value: '00000000000000000010'B
                },

                {
                  cn_DomainIdentity: cs_domain,
                  start_Value: '00000000000000000010'B
                }
              ],
              ue_RadioAccessCapability:
              {
                accessStratumReleaseIndicator: r99,
                pdcp_Capability:
                {
                  losslessSRNS_RelocationSupport: GcTRUE,
                  supportForRfc2507:
                  [
                    supported: by8192
                  ]
                },
                rlc_Capability:
                {
                  totalRLC_AM_BufferSize: kb50,
                  maximumRLC_WindowSize: mws2047,
                  maximumAM_EntityNumber: am6
                },
                transportChannelCapability:
                {
                  dl_TransChCapability:
                  {
                    maxNoBitsReceived: b5120,
                    maxConvCodeBitsReceived: b1280,
                    turboDecodingSupport:
                    [
                      supported: b5120
                    ],
                    maxSimultaneousTransChs: e8,
                    maxSimultaneousCCTrCH_Count: 1,
                    maxReceivedTransportBlocks: tb16,
                    maxNumberOfTFC: tfc96,
                    maxNumberOfTF: tf64
                  },
                  ul_TransChCapability:
                  {
                    maxNoBitsTransmitted: b3840,
                    maxConvCodeBitsTransmitted: b1280,
                    turboEncodingSupport:
                    [
                      supported: b3840
                    ],
                    maxSimultaneousTransChs: e8,
                    modeSpecificInfo:
                    [
                      fdd: NULL
                    ],
                    maxTransmittedBlocks: tb8,
                    maxNumberOfTFC: tfc32,
                    maxNumberOfTF: tf32
                  }
                },
                rf_Capability:
                {
                  fddRF_Capability:
                  {
                    ue_PowerClass: 4,
                    txRxFrequencySeparation: mhz190
                  },
                  tddRF_Capability: OMIT
                },
                physicalChannelCapability:
                {
                  fddPhysChCapability:
                  {
                    downlinkPhysChCapability:
                    {
                      maxNoDPCH_PDSCH_Codes: 3,
                      maxNoPhysChBitsReceived: b9600,
                      supportForSF_512: GcFALSE,
                      supportOfPDSCH: GcFALSE,
                      simultaneousSCCPCH_DPCH_Reception:
                      [
                        notSupported: NULL
                      ]
                    },
                    uplinkPhysChCapability:
                    {
                      maxNoDPDCH_BitsTransmitted: b2400,
                      supportOfPCPCH: GcFALSE
                    }
                  },
                  tddPhysChCapability: OMIT
                },
                ue_MultiModeRAT_Capability:
                {
                  multiRAT_CapabilityList:
                  {
                    supportOfGSM: GcFALSE,
                    supportOfMulticarrier: GcFALSE
                  },
                  multiModeCapability: fdd
                },
                securityCapability:
                {
                  cipheringAlgorithmCap: '0000000000000001'B,
                  integrityProtectionAlgorithmCap: '0000000000000010'B
                },
                ue_positioning_Capability:
                {
                  standaloneLocMethodsSupported: GcFALSE,
                  ue_BasedOTDOA_Supported: GcFALSE,
                  networkAssistedGPS_Supported: noNetworkAssistedGPS,
                  supportForUE_GPS_TimingOfCellFrames: GcFALSE,
                  supportForIPDL: GcFALSE
                },
                measurementCapability:
                {
                  downlinkCompressedMode:
                  {
                    fdd_Measurements: GcTRUE,
                    tdd_Measurements: OMIT,
                    gsm_Measurements:
                    {
                      gsm900: GcTRUE,
                      dcs1800: GcTRUE,
                      gsm1900: GcFALSE
                    },
                    multiCarrierMeasurements: GcFALSE
                  },
                  uplinkCompressedMode:
                  {
                    fdd_Measurements: GcTRUE,
                    tdd_Measurements: OMIT,
                    gsm_Measurements:
                    {
                      gsm900: GcTRUE,
                      dcs1800: GcTRUE,
                      gsm1900: GcFALSE
                    },
                    multiCarrierMeasurements: GcFALSE
                  }
                }
              },
              ue_RATSpecificCapability: OMIT,
              v370NonCriticalExtensions: OMIT
            }
          ]
        }
      ]
    }

TTCN PDU: RRC_DataInd

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      rB_Id: 3,
      ch: OMIT,
      sapId: OMIT,
      cN_Domain: 0,
      start: '00000000000000000010'B,
      msg: PDU:
      {
        skipIndicator: '0000'B,
        mMProtocolDiscriminator: '0101'B,
        msgType: '00001000'B,
        ciphKeySeqNum:
        {
          spare1: '0'B,
          keySeq: '000'B
        },
        locUpdType:
        {
          fOR: '0'B,
          spare1: '0'B,
          lUT: '10'B
        },
        locAreaId:
        {
          plmn: '00F110'O,
          lac: '0001'O
        },
        mSClsmk1:
        {
          spare1: '0'B,
          revLvl: '10'B,
          eSIND: '0'B,
          a5_1: '1'B,
          rFPwrCap: '111'B
        },
        mobileId:
        {
          iel: '05'O,
          iDigit1: '1111'B,
          oddEvenInd: '0'B,
          typeOfId: '100'B,
          otherDigits: '11223344'O
        },
        mSClsmk2:
        {
          iei: '00110011'B,
          iel: '03'O,
          spare1_1: '0'B,
          revLvl: '10'B,
          eSIND: '0'B,
          a5_1: '1'B,
          rFPwrCap: '111'B,
          spare1_2: '0'B,
          pSCap: '0'B,
          sSSI: '01'B,
          sMCap: '1'B,
          vBS: '0'B,
          vGCS: '0'B,
          fC: '0'B,
          cM3: '1'B,
          spare1_3: '0'B,
          lCSVA: '0'B,
          uCS2: '0'B,
          soLSA: '0'B,
          cMSP: '0'B,
          a5_3: '0'B,
          a5_2: '0'B
        }
      }
    }

TTCN PDU: RRC_DataReq

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      rB_Id: 3,
      ch: OMIT,
      sapId: OMIT,
      cN_Domain: 0,
      msg: PDU:
      {
        skipIndicator: '0000'B,
        mMProtocolDiscriminator: '0101'B,
        msgType: '00010010'B,
        spare4: '0000'B,
        ciphKeySeqNum:
        {
          spare1: '0'B,
          keySeq: '000'B
        },
        rAND: '01010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101'B,
        aUTN:
        {
          iei: '00100000'B,
          iel: '10'O,
          aUTN: '01100110000100010000000000110011001000101101110100000000000000000101010101000100011101110110011000010001000000000011001100100010'B
        }
      }
    }

TTCN PDU: Assignment:[3] tcv_AuthRs

(To search, click here and then press Ctrl+F)

    := PDU:
    {
      skipIndicator: '0000'B,
      mMProtocolDiscriminator: '0101'B,
      msgType: '01010100'B,
      authRsp: '01010101010001000111011101100110'B,
      authRspExt:
      {
        iei: '00100001'B,
        iel: '0C'O,
        rES: '000100010000000000110011001000101101110111001100111111111110111010011001100010001011101110101010'B
      }
    }

TTCN PDU: RRC_DataInd

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      rB_Id: 3,
      ch: OMIT,
      sapId: OMIT,
      cN_Domain: 0,
      start: OMIT,
      msg: PDU:
      {
        skipIndicator: '0000'B,
        mMProtocolDiscriminator: '0101'B,
        msgType: '01010100'B,
        authRsp: '01010101010001000111011101100110'B,
        authRspExt:
        {
          iei: '00100001'B,
          iel: '0C'O,
          rES: '000100010000000000110011001000101101110111001100111111111110111010011001100010001011101110101010'B
        }
      }
    }

TTCN PDU: CRLC_SecurityMode_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      rlcSecurityInfo:
      {
        cn_DomainIdentity: cs_domain,
        startValue: '00000000000000000000'B,
        cipheringKey: OMIT,
        integrityKey: '01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100'B,
        gsmCipheringKey: OMIT
      }
    }

TTCN PDU: CRLC_SetRRC_MessageSN_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: 0
      ],
      count_I_LSB_UL: OMIT,
      count_I_LSB_DL: 0
    }

TTCN PDU: CRLC_SetRRC_MessageSN_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 1
      ],
      count_I_LSB_UL: OMIT,
      count_I_LSB_DL: 0
    }

TTCN PDU: CRLC_SetRRC_MessageSN_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 2
      ],
      count_I_LSB_UL: OMIT,
      count_I_LSB_DL: 0
    }

TTCN PDU: CRLC_SetRRC_MessageSN_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 3
      ],
      count_I_LSB_UL: OMIT,
      count_I_LSB_DL: 0
    }

TTCN PDU: CRLC_SetRRC_MessageSN_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 4
      ],
      count_I_LSB_UL: OMIT,
      count_I_LSB_DL: 0
    }

TTCN PDU: CRLC_Integrity_Activate_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      cn_DomainIdentity: cs_domain,
      integrityActivationInfo:
      [
        integrityProtectionModeInfo:
        {
          integrityProtectionModeCommand:
          [
            startIntegrityProtection:
            {
              integrityProtInitNumber: '00001111000011110000111100001111'B
            }
          ],
          integrityProtectionAlgorithm: uia1
        }
      ]
    }

TTCN PDU: CRLC_Integrity_Activate_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      cn_DomainIdentity: cs_domain,
      integrityActivationInfo:
      [
        ul_IntegProtActivationInfo:
        [
          {
            rb_Identity: 2,
            rrc_MessageSequenceNumber: 0
          }
        ]
      ]
    }

TTCN PDU: RLC_AM_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 2
      ],
      confirmationRequest:
      [
        noConfirmationRequest: NULL
      ],
      aM_message:
      [
        dL_DCCH_Message: PDU:
        {
          integrityCheckInfo:
          {
            messageAuthenticationCode: '10000110000011011010000010001001'B,
            rrc_MessageSequenceNumber: 1
          },
          message:
          [
            securityModeCommand:
            [
              r3:
              {
                securityModeCommand_r3:
                {
                  rrc_TransactionIdentifier: 0,
                  securityCapability:
                  {
                    cipheringAlgorithmCap: '0000000000000001'B,
                    integrityProtectionAlgorithmCap: '0000000000000010'B
                  },
                  cipheringModeInfo: OMIT,
                  integrityProtectionModeInfo:
                  {
                    integrityProtectionModeCommand:
                    [
                      startIntegrityProtection:
                      {
                        integrityProtInitNumber: '00001111000011110000111100001111'B
                      }
                    ],
                    integrityProtectionAlgorithm: uia1
                  },
                  cn_DomainIdentity: cs_domain,
                  ue_SystemSpecificSecurityCap: OMIT
                },
                laterNonCriticalExtensions: OMIT
              }
            ]
          ]
        }
      ]
    }

TTCN PDU: RLC_AM_DATA_IND

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 2
      ],
      integrityResult:
      [
        integrityUsed: i_pass
      ],
      aM_message:
      [
        uL_DCCH_Message: PDU:
        {
          integrityCheckInfo:
          {
            messageAuthenticationCode: '10001011001000110111110011100010'B,
            rrc_MessageSequenceNumber: 1
          },
          message:
          [
            securityModeComplete:
            {
              rrc_TransactionIdentifier: 0,
              ul_IntegProtActivationInfo:
              {
                rrc_MessageSequenceNumberList:
                [
                  0,
                  0,
                  0,
                  0,
                  0
                ]
              },
              rb_UL_CiphActivationTimeInfo: OMIT,
              laterNonCriticalExtensions: OMIT
            }
          ]
        }
      ]
    }

TTCN PDU: CRLC_Integrity_Activate_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      cn_DomainIdentity: cs_domain,
      integrityActivationInfo:
      [
        ul_IntegProtActivationInfo:
        [
          {
            rb_Identity: 0,
            rrc_MessageSequenceNumber: 0
          },

          {
            rb_Identity: 1,
            rrc_MessageSequenceNumber: 0
          },

          {
            rb_Identity: 3,
            rrc_MessageSequenceNumber: 0
          },

          {
            rb_Identity: 4,
            rrc_MessageSequenceNumber: 0
          }
        ]
      ]
    }

TTCN PDU: RRC_DataReq

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      rB_Id: 3,
      ch: OMIT,
      sapId: OMIT,
      cN_Domain: 0,
      msg: PDU:
      {
        skipIndicator: '0000'B,
        mMProtocolDiscriminator: '0101'B,
        msgType: '00000010'B,
        locAreaId:
        {
          plmn: '00F110'O,
          lac: '0001'O
        },
        mobileId:
        {
          iei: '00010111'B,
          iel: '05'O,
          iDigit1: '1111'B,
          oddEvenInd: '0'B,
          typeOfId: '100'B,
          otherDigits: '11223344'O
        },
        followOnProceed: '10100001'B,
        cTSPerm: '10100010'B,
        equivalentPLMN: OMIT
      }
    }

TTCN PDU: RRC_DataInd

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      rB_Id: 3,
      ch: OMIT,
      sapId: OMIT,
      cN_Domain: 0,
      start: OMIT,
      msg: PDU:
      {
        skipIndicator: '0000'B,
        mMProtocolDiscriminator: '0101'B,
        msgType: '10011011'B
      }
    }

TTCN PDU: RLC_UM_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 1
      ],
      uM_message:
      [
        dL_DCCH_Message: PDU:
        {
          integrityCheckInfo:
          {
            messageAuthenticationCode: '11101100100111000001011111010011'B,
            rrc_MessageSequenceNumber: 1
          },
          message:
          [
            rrcConnectionRelease:
            [
              r3:
              {
                rrcConnectionRelease_r3:
                {
                  rrc_TransactionIdentifier: 0,
                  n_308: 1,
                  releaseCause: normalEvent,
                  rplmn_information: OMIT
                },
                laterNonCriticalExtensions: OMIT
              }
            ]
          ]
        }
      ],
      specialLI: GcFALSE
    }

TTCN PDU: RLC_UM_DATA_IND

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 1
      ],
      integrityResult:
      [
        integrityUsed: i_pass
      ],
      uM_message:
      [
        uL_DCCH_Message: PDU:
        {
          integrityCheckInfo:
          {
            messageAuthenticationCode: '11110111111000101100001011001110'B,
            rrc_MessageSequenceNumber: 1
          },
          message:
          [
            rrcConnectionReleaseComplete:
            {
              rrc_TransactionIdentifier: 0,
              errorIndication: OMIT,
              laterNonCriticalExtensions: OMIT
            }
          ]
        }
      ]
    }

TTCN PDU: RLC_UM_DATA_IND

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 1
      ],
      integrityResult:
      [
        integrityUsed: i_pass
      ],
      uM_message:
      [
        uL_DCCH_Message: PDU:
        {
          integrityCheckInfo:
          {
            messageAuthenticationCode: '10111001101000110000011111000000'B,
            rrc_MessageSequenceNumber: 2
          },
          message:
          [
            rrcConnectionReleaseComplete:
            {
              rrc_TransactionIdentifier: 0,
              errorIndication: OMIT,
              laterNonCriticalExtensions: OMIT
            }
          ]
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 1
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 2
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 3
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 4
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 1
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          sS_rlc_Info:
          {
            sS_ul_RLC_Mode:
            [
              dl_UM_RLC_Mode: NULL
            ],
            sS_dl_RLC_Mode:
            {
              dl_PayloadSize: 136,
              dl_RLCModeInfo:
              [
                ul_UM_RLC_Mode:
                {
                  transmissionRLC_Discard:
                  [
                    timerBasedNoExplicit: dt100
                  ]
                }
              ]
            }
          },
          rB_LogCH_Mapping:
          {
            uLlogicalChannelIdentity: 1,
            dLlogicalChannelIdentity: 1,
            logicalChannelType: OMIT,
            cn_DomainIdentity: OMIT
          }
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 2
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          sS_rlc_Info:
          {
            sS_ul_RLC_Mode:
            [
              dl_AM_RLC_Mode:
              {
                inSequenceDelivery: GcTRUE,
                receivingWindowSize: rw32,
                dl_RLC_StatusInfo:
                {
                  timerStatusProhibit: tsp200,
                  timerEPC: OMIT,
                  missingPDU_Indicator: GcTRUE,
                  timerStatusPeriodic: OMIT
                }
              }
            ],
            sS_dl_RLC_Mode:
            {
              dl_PayloadSize: 128,
              dl_RLCModeInfo:
              [
                ul_AM_RLC_Mode:
                {
                  transmissionRLC_Discard:
                  [
                    noDiscard: dat15
                  ],
                  transmissionWindowSize: tw32,
                  timerRST: tr500,
                  max_RST: rst1,
                  pollingInfo:
                  {
                    timerPollProhibit: tpp200,
                    timerPoll: tp200,
                    poll_PDU: OMIT,
                    poll_SDU: sdu1,
                    lastTransmissionPDU_Poll: GcTRUE,
                    lastRetransmissionPDU_Poll: GcTRUE,
                    pollWindow: pw99,
                    timerPollPeriodic: OMIT
                  }
                }
              ]
            }
          },
          rB_LogCH_Mapping:
          {
            uLlogicalChannelIdentity: 2,
            dLlogicalChannelIdentity: 2,
            logicalChannelType: OMIT,
            cn_DomainIdentity: OMIT
          }
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 3
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          sS_rlc_Info:
          {
            sS_ul_RLC_Mode:
            [
              dl_AM_RLC_Mode:
              {
                inSequenceDelivery: GcTRUE,
                receivingWindowSize: rw32,
                dl_RLC_StatusInfo:
                {
                  timerStatusProhibit: tsp200,
                  timerEPC: OMIT,
                  missingPDU_Indicator: GcTRUE,
                  timerStatusPeriodic: OMIT
                }
              }
            ],
            sS_dl_RLC_Mode:
            {
              dl_PayloadSize: 128,
              dl_RLCModeInfo:
              [
                ul_AM_RLC_Mode:
                {
                  transmissionRLC_Discard:
                  [
                    noDiscard: dat15
                  ],
                  transmissionWindowSize: tw32,
                  timerRST: tr500,
                  max_RST: rst1,
                  pollingInfo:
                  {
                    timerPollProhibit: tpp200,
                    timerPoll: tp200,
                    poll_PDU: OMIT,
                    poll_SDU: sdu1,
                    lastTransmissionPDU_Poll: GcTRUE,
                    lastRetransmissionPDU_Poll: GcTRUE,
                    pollWindow: pw99,
                    timerPollPeriodic: OMIT
                  }
                }
              ]
            }
          },
          rB_LogCH_Mapping:
          {
            uLlogicalChannelIdentity: 3,
            dLlogicalChannelIdentity: 3,
            logicalChannelType: OMIT,
            cn_DomainIdentity: OMIT
          }
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 4
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          sS_rlc_Info:
          {
            sS_ul_RLC_Mode:
            [
              dl_AM_RLC_Mode:
              {
                inSequenceDelivery: GcTRUE,
                receivingWindowSize: rw32,
                dl_RLC_StatusInfo:
                {
                  timerStatusProhibit: tsp200,
                  timerEPC: OMIT,
                  missingPDU_Indicator: GcTRUE,
                  timerStatusPeriodic: OMIT
                }
              }
            ],
            sS_dl_RLC_Mode:
            {
              dl_PayloadSize: 128,
              dl_RLCModeInfo:
              [
                ul_AM_RLC_Mode:
                {
                  transmissionRLC_Discard:
                  [
                    noDiscard: dat15
                  ],
                  transmissionWindowSize: tw32,
                  timerRST: tr500,
                  max_RST: rst1,
                  pollingInfo:
                  {
                    timerPollProhibit: tpp200,
                    timerPoll: tp200,
                    poll_PDU: OMIT,
                    poll_SDU: sdu1,
                    lastTransmissionPDU_Poll: GcTRUE,
                    lastRetransmissionPDU_Poll: GcTRUE,
                    pollWindow: pw99,
                    timerPollPeriodic: OMIT
                  }
                }
              ]
            }
          },
          rB_LogCH_Mapping:
          {
            uLlogicalChannelIdentity: 4,
            dLlogicalChannelIdentity: 4,
            logicalChannelType: OMIT,
            cn_DomainIdentity: OMIT
          }
        }
      ]
    }

TTCN PDU: AT_CmdCnf

(To search, click here and then press Ctrl+F)

    {
      result: OMIT,
      resultString: "<CR><LF>OK<CR><LF>",
      sMS_BlockMode: OMIT
    }

TTCN PDU: RLC_TR_DATA_IND

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: 0
      ],
      tM_message:
      [
        uL_CCCH_Message: PDU:
        {
          integrityCheckInfo: OMIT,
          message:
          [
            rrcConnectionRequest:
            {
              initialUE_Identity:
              [
                tmsi_and_LAI:
                {
                  tmsi: '00010001001000100011001101000100'B,
                  lai:
                  {
                    plmn_Identity:
                    {
                      mcc:
                      [
                        0,
                        0,
                        1
                      ],
                      mnc:
                      [
                        0,
                        1
                      ]
                    },
                    lac: '0000000000000001'B
                  }
                }
              ],
              establishmentCause: registration,
              protocolErrorIndicator: noError,
              measuredResultsOnRACH: OMIT,
              v3d0NonCriticalExtensions: OMIT
            }
          ]
        }
      ]
    }

TTCN PDU: RLC_UM_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: 0
      ],
      uM_message:
      [
        dL_CCCH_Message: PDU:
        {
          integrityCheckInfo: OMIT,
          message:
          [
            rrcConnectionSetup:
            [
              r3:
              {
                rrcConnectionSetup_r3:
                {
                  initialUE_Identity:
                  [
                    tmsi_and_LAI:
                    {
                      tmsi: '00010001001000100011001101000100'B,
                      lai:
                      {
                        plmn_Identity:
                        {
                          mcc:
                          [
                            0,
                            0,
                            1
                          ],
                          mnc:
                          [
                            0,
                            1
                          ]
                        },
                        lac: '0000000000000001'B
                      }
                    }
                  ],
                  rrc_TransactionIdentifier: 0,
                  activationTime: OMIT,
                  new_U_RNTI:
                  {
                    srnc_Identity: '000000000001'B,
                    s_RNTI: '00000000000000000001'B
                  },
                  new_c_RNTI: OMIT,
                  rrc_StateIndicator: cell_DCH,
                  utran_DRX_CycleLengthCoeff: 9,
                  capabilityUpdateRequirement:
                  {
                    ue_RadioCapabilityFDDUpdateRequirement: GcTRUE,
                    ue_RadioCapabilityTDDUpdateRequirement: GcFALSE,
                    systemSpecificCapUpdateReqList:
                    [
                      gsm
                    ]
                  },
                  srb_InformationSetupList:
                  [
                    {
                      rb_Identity: OMIT,
                      rlc_InfoChoice:
                      [
                        rlc_Info:
                        {
                          ul_RLC_Mode:
                          [
                            ul_UM_RLC_Mode:
                            {
                              transmissionRLC_Discard: OMIT
                            }
                          ],
                          dl_RLC_Mode:
                          [
                            dl_UM_RLC_Mode: NULL
                          ]
                        }
                      ],
                      rb_MappingInfo:
                      [
                        {
                          ul_LogicalChannelMappings:
                          [
                            oneLogicalChannel:
                            {
                              ul_TransportChannelType:
                              [
                                dch: 5
                              ],
                              logicalChannelIdentity: 1,
                              rlc_SizeList:
                              [
                                configured: NULL
                              ],
                              mac_LogicalChannelPriority: 1
                            }
                          ],
                          dl_LogicalChannelMappingList:
                          [
                            {
                              dl_TransportChannelType:
                              [
                                dch: 10
                              ],
                              logicalChannelIdentity: 1
                            }
                          ]
                        },

                        {
                          ul_LogicalChannelMappings:
                          [
                            oneLogicalChannel:
                            {
                              ul_TransportChannelType:
                              [
                                rach: NULL
                              ],
                              logicalChannelIdentity: 1,
                              rlc_SizeList:
                              [
                                explicitList:
                                [
                                  {
                                    rlc_SizeIndex: 1
                                  }
                                ]
                              ],
                              mac_LogicalChannelPriority: 1
                            }
                          ],
                          dl_LogicalChannelMappingList:
                          [
                            {
                              dl_TransportChannelType:
                              [
                                fach: NULL
                              ],
                              logicalChannelIdentity: 1
                            }
                          ]
                        }
                      ]
                    },

                    {
                      rb_Identity: OMIT,
                      rlc_InfoChoice:
                      [
                        rlc_Info:
                        {
                          ul_RLC_Mode:
                          [
                            ul_AM_RLC_Mode:
                            {
                              transmissionRLC_Discard:
                              [
                                noDiscard: dat15
                              ],
                              transmissionWindowSize: tw32,
                              timerRST: tr500,
                              max_RST: rst1,
                              pollingInfo:
                              {
                                timerPollProhibit: tpp200,
                                timerPoll: tp200,
                                poll_PDU: OMIT,
                                poll_SDU: sdu1,
                                lastTransmissionPDU_Poll: GcTRUE,
                                lastRetransmissionPDU_Poll: GcTRUE,
                                pollWindow: pw99,
                                timerPollPeriodic: OMIT
                              }
                            }
                          ],
                          dl_RLC_Mode:
                          [
                            dl_AM_RLC_Mode:
                            {
                              inSequenceDelivery: GcTRUE,
                              receivingWindowSize: rw32,
                              dl_RLC_StatusInfo:
                              {
                                timerStatusProhibit: tsp200,
                                timerEPC: OMIT,
                                missingPDU_Indicator: GcTRUE,
                                timerStatusPeriodic: OMIT
                              }
                            }
                          ]
                        }
                      ],
                      rb_MappingInfo:
                      [
                        {
                          ul_LogicalChannelMappings:
                          [
                            oneLogicalChannel:
                            {
                              ul_TransportChannelType:
                              [
                                dch: 5
                              ],
                              logicalChannelIdentity: 2,
                              rlc_SizeList:
                              [
                                configured: NULL
                              ],
                              mac_LogicalChannelPriority: 2
                            }
                          ],
                          dl_LogicalChannelMappingList:
                          [
                            {
                              dl_TransportChannelType:
                              [
                                dch: 10
                              ],
                              logicalChannelIdentity: 2
                            }
                          ]
                        },

                        {
                          ul_LogicalChannelMappings:
                          [
                            oneLogicalChannel:
                            {
                              ul_TransportChannelType:
                              [
                                rach: NULL
                              ],
                              logicalChannelIdentity: 2,
                              rlc_SizeList:
                              [
                                explicitList:
                                [
                                  {
                                    rlc_SizeIndex: 1
                                  }
                                ]
                              ],
                              mac_LogicalChannelPriority: 2
                            }
                          ],
                          dl_LogicalChannelMappingList:
                          [
                            {
                              dl_TransportChannelType:
                              [
                                fach: NULL
                              ],
                              logicalChannelIdentity: 2
                            }
                          ]
                        }
                      ]
                    },

                    {
                      rb_Identity: OMIT,
                      rlc_InfoChoice:
                      [
                        rlc_Info:
                        {
                          ul_RLC_Mode:
                          [
                            ul_AM_RLC_Mode:
                            {
                              transmissionRLC_Discard:
                              [
                                noDiscard: dat15
                              ],
                              transmissionWindowSize: tw32,
                              timerRST: tr500,
                              max_RST: rst1,
                              pollingInfo:
                              {
                                timerPollProhibit: tpp200,
                                timerPoll: tp200,
                                poll_PDU: OMIT,
                                poll_SDU: sdu1,
                                lastTransmissionPDU_Poll: GcTRUE,
                                lastRetransmissionPDU_Poll: GcTRUE,
                                pollWindow: pw99,
                                timerPollPeriodic: OMIT
                              }
                            }
                          ],
                          dl_RLC_Mode:
                          [
                            dl_AM_RLC_Mode:
                            {
                              inSequenceDelivery: GcTRUE,
                              receivingWindowSize: rw32,
                              dl_RLC_StatusInfo:
                              {
                                timerStatusProhibit: tsp200,
                                timerEPC: OMIT,
                                missingPDU_Indicator: GcTRUE,
                                timerStatusPeriodic: OMIT
                              }
                            }
                          ]
                        }
                      ],
                      rb_MappingInfo:
                      [
                        {
                          ul_LogicalChannelMappings:
                          [
                            oneLogicalChannel:
                            {
                              ul_TransportChannelType:
                              [
                                dch: 5
                              ],
                              logicalChannelIdentity: 3,
                              rlc_SizeList:
                              [
                                configured: NULL
                              ],
                              mac_LogicalChannelPriority: 3
                            }
                          ],
                          dl_LogicalChannelMappingList:
                          [
                            {
                              dl_TransportChannelType:
                              [
                                dch: 10
                              ],
                              logicalChannelIdentity: 3
                            }
                          ]
                        },

                        {
                          ul_LogicalChannelMappings:
                          [
                            oneLogicalChannel:
                            {
                              ul_TransportChannelType:
                              [
                                rach: NULL
                              ],
                              logicalChannelIdentity: 3,
                              rlc_SizeList:
                              [
                                explicitList:
                                [
                                  {
                                    rlc_SizeIndex: 1
                                  }
                                ]
                              ],
                              mac_LogicalChannelPriority: 3
                            }
                          ],
                          dl_LogicalChannelMappingList:
                          [
                            {
                              dl_TransportChannelType:
                              [
                                fach: NULL
                              ],
                              logicalChannelIdentity: 3
                            }
                          ]
                        }
                      ]
                    },

                    {
                      rb_Identity: OMIT,
                      rlc_InfoChoice:
                      [
                        rlc_Info:
                        {
                          ul_RLC_Mode:
                          [
                            ul_AM_RLC_Mode:
                            {
                              transmissionRLC_Discard:
                              [
                                noDiscard: dat15
                              ],
                              transmissionWindowSize: tw32,
                              timerRST: tr500,
                              max_RST: rst1,
                              pollingInfo:
                              {
                                timerPollProhibit: tpp200,
                                timerPoll: tp200,
                                poll_PDU: OMIT,
                                poll_SDU: sdu1,
                                lastTransmissionPDU_Poll: GcTRUE,
                                lastRetransmissionPDU_Poll: GcTRUE,
                                pollWindow: pw99,
                                timerPollPeriodic: OMIT
                              }
                            }
                          ],
                          dl_RLC_Mode:
                          [
                            dl_AM_RLC_Mode:
                            {
                              inSequenceDelivery: GcTRUE,
                              receivingWindowSize: rw32,
                              dl_RLC_StatusInfo:
                              {
                                timerStatusProhibit: tsp200,
                                timerEPC: OMIT,
                                missingPDU_Indicator: GcTRUE,
                                timerStatusPeriodic: OMIT
                              }
                            }
                          ]
                        }
                      ],
                      rb_MappingInfo:
                      [
                        {
                          ul_LogicalChannelMappings:
                          [
                            oneLogicalChannel:
                            {
                              ul_TransportChannelType:
                              [
                                dch: 5
                              ],
                              logicalChannelIdentity: 4,
                              rlc_SizeList:
                              [
                                configured: NULL
                              ],
                              mac_LogicalChannelPriority: 4
                            }
                          ],
                          dl_LogicalChannelMappingList:
                          [
                            {
                              dl_TransportChannelType:
                              [
                                dch: 10
                              ],
                              logicalChannelIdentity: 4
                            }
                          ]
                        },

                        {
                          ul_LogicalChannelMappings:
                          [
                            oneLogicalChannel:
                            {
                              ul_TransportChannelType:
                              [
                                rach: NULL
                              ],
                              logicalChannelIdentity: 4,
                              rlc_SizeList:
                              [
                                explicitList:
                                [
                                  {
                                    rlc_SizeIndex: 1
                                  }
                                ]
                              ],
                              mac_LogicalChannelPriority: 4
                            }
                          ],
                          dl_LogicalChannelMappingList:
                          [
                            {
                              dl_TransportChannelType:
                              [
                                fach: NULL
                              ],
                              logicalChannelIdentity: 4
                            }
                          ]
                        }
                      ]
                    }
                  ],
                  ul_CommonTransChInfo:
                  {
                    tfc_Subset: OMIT,
                    prach_TFCS: OMIT,
                    modeSpecificInfo:
                    [
                      fdd:
                      {
                        ul_TFCS:
                        [
                          normalTFCI_Signalling:
                          [
                            complete:
                            {
                              ctfcSize:
                              [
                                ctfc2Bit:
                                [
                                  {
                                    ctfc2: 0,
                                    powerOffsetInformation:
                                    {
                                      gainFactorInformation:
                                      [
                                        computedGainFactors: 0
                                      ],
                                      powerOffsetPp_m: OMIT
                                    }
                                  },

                                  {
                                    ctfc2: 1,
                                    powerOffsetInformation:
                                    {
                                      gainFactorInformation:
                                      [
                                        signalledGainFactors:
                                        {
                                          modeSpecificInfo:
                                          [
                                            fdd:
                                            {
                                              gainFactorBetaC: 11
                                            }
                                          ],
                                          gainFactorBetaD: 15,
                                          referenceTFC_ID: 0
                                        }
                                      ],
                                      powerOffsetPp_m: OMIT
                                    }
                                  }
                                ]
                              ]
                            }
                          ]
                        ]
                      }
                    ]
                  },
                  ul_AddReconfTransChInfoList:
                  [
                    {
                      ul_TransportChannelType: dch,
                      transportChannelIdentity: 5,
                      transportFormatSet:
                      [
                        dedicatedTransChTFS:
                        {
                          tti:
                          [
                            tti10:
                            [
                              {
                                rlc_Size:
                                [
                                  bitMode:
                                  [
                                    sizeType2:
                                    {
                                      part1: 2,
                                      part2: OMIT
                                    }
                                  ]
                                ],
                                numberOfTbSizeList:
                                [
                                  [
                                    zero: NULL
                                  ],

                                  [
                                    one: NULL
                                  ]
                                ],
                                logicalChannelList:
                                [
                                  allSizes: NULL
                                ]
                              }
                            ]
                          ],
                          semistaticTF_Information:
                          {
                            channelCodingType:
                            [
                              convolutional: third
                            ],
                            rateMatchingAttribute# 192 # crc_Size# crc16
                          }
                        }
                      ]
                    }
                  ]
                  # dl_CommonTransChInfo#
                  {
                    sccpch_TFCS# OMIT# modeSpecificInfo#
                    [
                      fdd#
                      {
                        dl_Parameters#
                        [
                          sameAsUL# NULL
                        ]
                      }
                    ]
                  }
                  # dl_AddReconfTransChInfoList#
                  [
                    {
                      dl_TransportChannelType# dch# dl_transportChannelIdentity# 10 # tfs_SignallingMode#
                      [
                        sameAsULTrCH#
                        {
                          ul_TransportChannelType# dch# ul_TransportChannelIdentity# 5
                        }
                      ]
                      # dch_QualityTarget#
                      {
                        bler_QualityValue# #20
                      }
                      # dummy# OMIT
                    }
                  ]
                  # frequencyInfo# OMIT# maxAllowedUL_TX_Power# OMIT# ul_ChannelRequirement#
                  [
                    ul_DPCH_Info#
                    {
                      ul_DPCH_PowerControlInfo#
                      [
                        fdd#
                        {
                          dpcch_PowerOffset# #40 # pc_Preamble# 1 # sRB_delay# 7 # powerControlAlgorithm#
                          [
                            algorithm1# 1
                          ]
                        }
                      ]
                      # modeSpecificInfo#
                      [
                        fdd#
                        {
                          scramblingCodeType# longSC# scramblingCode# 0 # numberOfDPDCH# OMIT# spreadingFactor# sf64# tfci_Existence# GcTRUE # numberOfFBI_Bits# OMIT# puncturingLimit# pl1
                        }
                      ]
                    }
                  ]
                  # dl_CommonInformation#
                  {
                    dl_DPCH_InfoCommon#
                    {
                      cfnHandling#
                      [
                        initialise#
                        {
                          cfntargetsfnframeoffset# OMIT
                        }
                      ]
                      # modeSpecificInfo#
                      [
                        fdd#
                        {
                          dl_DPCH_PowerControlInfo#
                          {
                            modeSpecificInfo#
                            [
                              fdd#
                              {
                                dpc_Mode# singleTPC
                              }
                            ]
                          }
                          # powerOffsetPilot_pdpdch# 0 # dl_rate_matching_restriction# OMIT# spreadingFactorAndPilot#
                          [
                            sfd128# pb4
                          ]
                          # positionFixedOrFlexible# fixed# tfci_Existence# GcFALSE
                        }
                      ]
                    }
                    # modeSpecificInfo#
                    [
                      fdd#
                      {
                        defaultDPCH_OffsetValue# 0 # dpch_CompressedModeInfo# OMIT# tx_DiversityMode# noDiversity# ssdt_Information# OMIT
                      }
                    ]
                  }
                  # dl_InformationPerRL_List#
                  [
                    {
                      modeSpecificInfo#
                      [
                        fdd#
                        {
                          primaryCPICH_Info#
                          {
                            primaryScramblingCode# 100
                          }
                          # pdsch_SHO_DCH_Info# OMIT# pdsch_CodeMapping# OMIT
                        }
                      ]
                      # dl_DPCH_InfoPerRL#
                      [
                        fdd#
                        {
                          pCPICH_UsageForChannelEst# mayBeUsed# dpch_FrameOffset# 0 # secondaryCPICH_Info# OMIT# dl_ChannelisationCodeList#
                          [
                            {
                              secondaryScramblingCode# 1 # sf_AndCodeNumber#
                              [
                                sf128# 0
                              ]
                              # scramblingCodeChange# noCodeChange
                            }
                          ]
                          # tpc_CombinationIndex# 0 # ssdt_CellIdentity# OMIT# closedLoopTimingAdjMode# OMIT
                        }
                      ]
                      # sccpch_InfoforFACH# OMIT
                    }
                  ]
                }
                # laterNonCriticalExtensions# OMIT
              }
            ]
          ]
        }
      ]
      # specialLI# GcTRUE
    }

TTCN PDU: RLC_AM_DATA_IND

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 2
      ],
      integrityResult:
      [
        integrityUsed: i_pass
      ],
      aM_message:
      [
        uL_DCCH_Message: PDU:
        {
          integrityCheckInfo: OMIT,
          message:
          [
            rrcConnectionSetupComplete:
            {
              rrc_TransactionIdentifier: 0,
              startList:
              [
                {
                  cn_DomainIdentity: ps_domain,
                  start_Value: '00000000000000000010'B
                },

                {
                  cn_DomainIdentity: cs_domain,
                  start_Value: '00000000000000000010'B
                }
              ],
              ue_RadioAccessCapability:
              {
                accessStratumReleaseIndicator: r99,
                pdcp_Capability:
                {
                  losslessSRNS_RelocationSupport: GcTRUE,
                  supportForRfc2507:
                  [
                    supported: by8192
                  ]
                },
                rlc_Capability:
                {
                  totalRLC_AM_BufferSize: kb50,
                  maximumRLC_WindowSize: mws2047,
                  maximumAM_EntityNumber: am6
                },
                transportChannelCapability:
                {
                  dl_TransChCapability:
                  {
                    maxNoBitsReceived: b5120,
                    maxConvCodeBitsReceived: b1280,
                    turboDecodingSupport:
                    [
                      supported: b5120
                    ],
                    maxSimultaneousTransChs: e8,
                    maxSimultaneousCCTrCH_Count: 1,
                    maxReceivedTransportBlocks: tb16,
                    maxNumberOfTFC: tfc96,
                    maxNumberOfTF: tf64
                  },
                  ul_TransChCapability:
                  {
                    maxNoBitsTransmitted: b3840,
                    maxConvCodeBitsTransmitted: b1280,
                    turboEncodingSupport:
                    [
                      supported: b3840
                    ],
                    maxSimultaneousTransChs: e8,
                    modeSpecificInfo:
                    [
                      fdd: NULL
                    ],
                    maxTransmittedBlocks: tb8,
                    maxNumberOfTFC: tfc32,
                    maxNumberOfTF: tf32
                  }
                },
                rf_Capability:
                {
                  fddRF_Capability:
                  {
                    ue_PowerClass: 4,
                    txRxFrequencySeparation: mhz190
                  },
                  tddRF_Capability: OMIT
                },
                physicalChannelCapability:
                {
                  fddPhysChCapability:
                  {
                    downlinkPhysChCapability:
                    {
                      maxNoDPCH_PDSCH_Codes: 3,
                      maxNoPhysChBitsReceived: b9600,
                      supportForSF_512: GcFALSE,
                      supportOfPDSCH: GcFALSE,
                      simultaneousSCCPCH_DPCH_Reception:
                      [
                        notSupported: NULL
                      ]
                    },
                    uplinkPhysChCapability:
                    {
                      maxNoDPDCH_BitsTransmitted: b2400,
                      supportOfPCPCH: GcFALSE
                    }
                  },
                  tddPhysChCapability: OMIT
                },
                ue_MultiModeRAT_Capability:
                {
                  multiRAT_CapabilityList:
                  {
                    supportOfGSM: GcFALSE,
                    supportOfMulticarrier: GcFALSE
                  },
                  multiModeCapability: fdd
                },
                securityCapability:
                {
                  cipheringAlgorithmCap: '0000000000000001'B,
                  integrityProtectionAlgorithmCap: '0000000000000010'B
                },
                ue_positioning_Capability:
                {
                  standaloneLocMethodsSupported: GcFALSE,
                  ue_BasedOTDOA_Supported: GcFALSE,
                  networkAssistedGPS_Supported: noNetworkAssistedGPS,
                  supportForUE_GPS_TimingOfCellFrames: GcFALSE,
                  supportForIPDL: GcFALSE
                },
                measurementCapability:
                {
                  downlinkCompressedMode:
                  {
                    fdd_Measurements: GcTRUE,
                    tdd_Measurements: OMIT,
                    gsm_Measurements:
                    {
                      gsm900: GcTRUE,
                      dcs1800: GcTRUE,
                      gsm1900: GcFALSE
                    },
                    multiCarrierMeasurements: GcFALSE
                  },
                  uplinkCompressedMode:
                  {
                    fdd_Measurements: GcTRUE,
                    tdd_Measurements: OMIT,
                    gsm_Measurements:
                    {
                      gsm900: GcTRUE,
                      dcs1800: GcTRUE,
                      gsm1900: GcFALSE
                    },
                    multiCarrierMeasurements: GcFALSE
                  }
                }
              },
              ue_RATSpecificCapability: OMIT,
              v370NonCriticalExtensions: OMIT
            }
          ]
        }
      ]
    }

TTCN PDU: Assignment:[33] tcv_TmpAttachRe

(To search, click here and then press Ctrl+F)

    := PDU:
    {
      skipIndicator: '0000'B,
      gMMProtocolDiscriminator: '1000'B,
      msgType: '00000001'B,
      msNetworkCap:
      {
        iel: '02'O,
        value: 'E540'O
      },
      gprsCiphKeySeqNo:
      {
        spare1: '0'B,
        keySeq: '001'B
      },
      attachType:
      {
        for: '0'B,
        type: '011'B
      },
      drxParameter:
      {
        splitPGcycleCode: '00000111'B,
        cnDRXcoef: '0000'B,
        splitOnCCCH: '0'B,
        nonDRXtimer: '010'B
      },
      ptmsiORimsi:
      {
        iel: '05'O,
        iDigit1: '1111'B,
        oddEvenInd: '0'B,
        typeOfId: '100'B,
        otherDigits: '12345678'O
      },
      oldRAI:
      {
        plmn: '00F110'O,
        lac: '0001'O,
        rac: '05'O
      },
      msRadioAccessCap:
      {
        iel: '0A'O,
        value: '14F382334C03263CA060'O
      },
      oldPTMSI_Signature: OMIT,
      readyTimer:
      {
        iei: '00010111'B,
        unit: '000'B,
        value: '10110'B
      },
      tmsiStatus: OMIT
    }

TTCN PDU: RRC_DataInd

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      rB_Id: 3,
      ch: OMIT,
      sapId: OMIT,
      cN_Domain: 1,
      start: '00000000000000000010'B,
      msg: PDU:
      {
        skipIndicator: '0000'B,
        gMMProtocolDiscriminator: '1000'B,
        msgType: '00000001'B,
        msNetworkCap:
        {
          iel: '02'O,
          value: 'E540'O
        },
        gprsCiphKeySeqNo:
        {
          spare1: '0'B,
          keySeq: '001'B
        },
        attachType:
        {
          for: '0'B,
          type: '011'B
        },
        drxParameter:
        {
          splitPGcycleCode: '00000111'B,
          cnDRXcoef: '0000'B,
          splitOnCCCH: '0'B,
          nonDRXtimer: '010'B
        },
        ptmsiORimsi:
        {
          iel: '05'O,
          iDigit1: '1111'B,
          oddEvenInd: '0'B,
          typeOfId: '100'B,
          otherDigits: '12345678'O
        },
        oldRAI:
        {
          plmn: '00F110'O,
          lac: '0001'O,
          rac: '05'O
        },
        msRadioAccessCap:
        {
          iel: '0A'O,
          value: '14F382334C03263CA060'O
        },
        oldPTMSI_Signature: OMIT,
        readyTimer:
        {
          iei: '00010111'B,
          unit: '000'B,
          value: '10110'B
        },
        tmsiStatus: OMIT
      }
    }

TTCN PDU: RRC_DataReq

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      rB_Id: 3,
      ch: OMIT,
      sapId: OMIT,
      cN_Domain: 1,
      msg: PDU:
      {
        skipIndicator: '0000'B,
        gMMProtocolDiscriminator: '1000'B,
        msgType: '00010010'B,
        imeisvReq:
        {
          spare1: '0'B,
          value: '000'B
        },
        ciphAlgorithm:
        {
          spare1: '0'B,
          algorithm: '001'B
        },
        acRefNo:
        {
          value: '0011'B
        },
        forceToStandby:
        {
          spare: '0'B,
          value: '000'B
        },
        authRand:
        {
          iei: '00100001'B,
          randValue: '01010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101'B
        },
        gprsCiphKeySeqNo:
        {
          iei: '1000'B,
          spare1: '0'B,
          keySeq: '000'B
        },
        aUTN:
        {
          iei: '00101000'B,
          iel: '10'O,
          aUTN: '01100110000100010000000000110011001000101101110100000000000000000101010101000100011101110110011000010001000000000011001100100010'B
        }
      }
    }

TTCN PDU: Assignment:[3] tcv_TmpAuthAndCiphRs

(To search, click here and then press Ctrl+F)

    := PDU:
    {
      skipIndicator: '0000'B,
      gMMProtocolDiscriminator: '1000'B,
      msgType: '00010011'B,
      spare4: '0000'B,
      acRefNo:
      {
        value: '0011'B
      },
      authRsp:
      {
        iei: '00100010'B,
        value: '01010101010001000111011101100110'B
      },
      imeisv: OMIT,
      authRspExt:
      {
        iei: '00101001'B,
        iel: '0C'O,
        rES: '000100010000000000110011001000101101110111001100111111111110111010011001100010001011101110101010'B
      }
    }

TTCN PDU: RRC_DataInd

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      rB_Id: 3,
      ch: OMIT,
      sapId: OMIT,
      cN_Domain: 1,
      start: OMIT,
      msg: PDU:
      {
        skipIndicator: '0000'B,
        gMMProtocolDiscriminator: '1000'B,
        msgType: '00010011'B,
        spare4: '0000'B,
        acRefNo:
        {
          value: '0011'B
        },
        authRsp:
        {
          iei: '00100010'B,
          value: '01010101010001000111011101100110'B
        },
        imeisv: OMIT,
        authRspExt:
        {
          iei: '00101001'B,
          iel: '0C'O,
          rES: '000100010000000000110011001000101101110111001100111111111110111010011001100010001011101110101010'B
        }
      }
    }

TTCN PDU: CRLC_SecurityMode_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      rlcSecurityInfo:
      {
        cn_DomainIdentity: ps_domain,
        startValue: '00000000000000000000'B,
        cipheringKey: OMIT,
        integrityKey: '01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100'B,
        gsmCipheringKey: OMIT
      }
    }

TTCN PDU: CRLC_SetRRC_MessageSN_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: 0
      ],
      count_I_LSB_UL: OMIT,
      count_I_LSB_DL: 0
    }

TTCN PDU: CRLC_SetRRC_MessageSN_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 1
      ],
      count_I_LSB_UL: OMIT,
      count_I_LSB_DL: 0
    }

TTCN PDU: CRLC_SetRRC_MessageSN_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 2
      ],
      count_I_LSB_UL: OMIT,
      count_I_LSB_DL: 0
    }

TTCN PDU: CRLC_SetRRC_MessageSN_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 3
      ],
      count_I_LSB_UL: OMIT,
      count_I_LSB_DL: 0
    }

TTCN PDU: CRLC_SetRRC_MessageSN_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 4
      ],
      count_I_LSB_UL: OMIT,
      count_I_LSB_DL: 0
    }

TTCN PDU: CRLC_Integrity_Activate_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      cn_DomainIdentity: ps_domain,
      integrityActivationInfo:
      [
        integrityProtectionModeInfo:
        {
          integrityProtectionModeCommand:
          [
            startIntegrityProtection:
            {
              integrityProtInitNumber: '00001111000011110000111100001111'B
            }
          ],
          integrityProtectionAlgorithm: uia1
        }
      ]
    }

TTCN PDU: CRLC_Integrity_Activate_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      cn_DomainIdentity: ps_domain,
      integrityActivationInfo:
      [
        ul_IntegProtActivationInfo:
        [
          {
            rb_Identity: 2,
            rrc_MessageSequenceNumber: 0
          }
        ]
      ]
    }

TTCN PDU: RLC_AM_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 2
      ],
      confirmationRequest:
      [
        noConfirmationRequest: NULL
      ],
      aM_message:
      [
        dL_DCCH_Message: PDU:
        {
          integrityCheckInfo:
          {
            messageAuthenticationCode: '00101001110000010111010101011011'B,
            rrc_MessageSequenceNumber: 1
          },
          message:
          [
            securityModeCommand:
            [
              r3:
              {
                securityModeCommand_r3:
                {
                  rrc_TransactionIdentifier: 0,
                  securityCapability:
                  {
                    cipheringAlgorithmCap: '0000000000000001'B,
                    integrityProtectionAlgorithmCap: '0000000000000010'B
                  },
                  cipheringModeInfo: OMIT,
                  integrityProtectionModeInfo:
                  {
                    integrityProtectionModeCommand:
                    [
                      startIntegrityProtection:
                      {
                        integrityProtInitNumber: '00001111000011110000111100001111'B
                      }
                    ],
                    integrityProtectionAlgorithm: uia1
                  },
                  cn_DomainIdentity: ps_domain,
                  ue_SystemSpecificSecurityCap: OMIT
                },
                laterNonCriticalExtensions: OMIT
              }
            ]
          ]
        }
      ]
    }

TTCN PDU: RLC_AM_DATA_IND

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 2
      ],
      integrityResult:
      [
        integrityUsed: i_pass
      ],
      aM_message:
      [
        uL_DCCH_Message: PDU:
        {
          integrityCheckInfo:
          {
            messageAuthenticationCode: '10001011001000110111110011100010'B,
            rrc_MessageSequenceNumber: 1
          },
          message:
          [
            securityModeComplete:
            {
              rrc_TransactionIdentifier: 0,
              ul_IntegProtActivationInfo:
              {
                rrc_MessageSequenceNumberList:
                [
                  0,
                  0,
                  0,
                  0,
                  0
                ]
              },
              rb_UL_CiphActivationTimeInfo: OMIT,
              laterNonCriticalExtensions: OMIT
            }
          ]
        }
      ]
    }

TTCN PDU: CRLC_Integrity_Activate_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      cn_DomainIdentity: ps_domain,
      integrityActivationInfo:
      [
        ul_IntegProtActivationInfo:
        [
          {
            rb_Identity: 0,
            rrc_MessageSequenceNumber: 0
          },

          {
            rb_Identity: 1,
            rrc_MessageSequenceNumber: 0
          },

          {
            rb_Identity: 3,
            rrc_MessageSequenceNumber: 0
          },

          {
            rb_Identity: 4,
            rrc_MessageSequenceNumber: 0
          }
        ]
      ]
    }

TTCN PDU: RRC_DataReq

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      rB_Id: 3,
      ch: OMIT,
      sapId: OMIT,
      cN_Domain: 1,
      msg: PDU:
      {
        skipIndicator: '0000'B,
        gMMProtocolDiscriminator: '1000'B,
        msgType: '00000010'B,
        forceToStandby:
        {
          spare: '0'B,
          value: '000'B
        },
        attachResult:
        {
          spare: '0'B,
          result: '011'B
        },
        periodicRAupdateTimer:
        {
          unit: '111'B,
          value: '00000'B
        },
        spare: '0000'B,
        radioPrioSMS:
        {
          spare: '0'B,
          value: '100'B
        },
        rai:
        {
          plmn: '00F110'O,
          lac: '0001'O,
          rac: '05'O
        },
        ptmsiSignature:
        {
          iei: '00011001'B,
          value: 'AB1234'O
        },
        negReadyTimer: OMIT,
        allocatedPTMSI:
        {
          iei: '00011000'B,
          iel: '05'O,
          iDigit1: '1111'B,
          oddEvenInd: '0'B,
          typeOfId: '100'B,
          otherDigits: '12345678'O
        },
        msIdentity:
        {
          iei: '00100011'B,
          iel: '05'O,
          iDigit1: '1111'B,
          oddEvenInd: '0'B,
          typeOfId: '100'B,
          otherDigits: '11223344'O
        },
        gmmCause: OMIT,
        t3302Value: OMIT,
        cellNotification: OMIT,
        equivalentPLMN: OMIT
      }
    }

TTCN PDU: RRC_DataInd

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      rB_Id: 3,
      ch: OMIT,
      sapId: OMIT,
      cN_Domain: 1,
      start: OMIT,
      msg: PDU:
      {
        skipIndicator: '0000'B,
        gMMProtocolDiscriminator: '1000'B,
        msgType: '00000011'B
      }
    }

TTCN PDU: RLC_UM_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 1
      ],
      uM_message:
      [
        dL_DCCH_Message: PDU:
        {
          integrityCheckInfo:
          {
            messageAuthenticationCode: '11101100100111000001011111010011'B,
            rrc_MessageSequenceNumber: 1
          },
          message:
          [
            rrcConnectionRelease:
            [
              r3:
              {
                rrcConnectionRelease_r3:
                {
                  rrc_TransactionIdentifier: 0,
                  n_308: 1,
                  releaseCause: normalEvent,
                  rplmn_information: OMIT
                },
                laterNonCriticalExtensions: OMIT
              }
            ]
          ]
        }
      ],
      specialLI: GcFALSE
    }

TTCN PDU: RLC_UM_DATA_IND

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 1
      ],
      integrityResult:
      [
        integrityUsed: i_pass
      ],
      uM_message:
      [
        uL_DCCH_Message: PDU:
        {
          integrityCheckInfo:
          {
            messageAuthenticationCode: '11110111111000101100001011001110'B,
            rrc_MessageSequenceNumber: 1
          },
          message:
          [
            rrcConnectionReleaseComplete:
            {
              rrc_TransactionIdentifier: 0,
              errorIndication: OMIT,
              laterNonCriticalExtensions: OMIT
            }
          ]
        }
      ]
    }

TTCN PDU: RLC_UM_DATA_IND

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 1
      ],
      integrityResult:
      [
        integrityUsed: i_pass
      ],
      uM_message:
      [
        uL_DCCH_Message: PDU:
        {
          integrityCheckInfo:
          {
            messageAuthenticationCode: '10111001101000110000011111000000'B,
            rrc_MessageSequenceNumber: 2
          },
          message:
          [
            rrcConnectionReleaseComplete:
            {
              rrc_TransactionIdentifier: 0,
              errorIndication: OMIT,
              laterNonCriticalExtensions: OMIT
            }
          ]
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 1
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 2
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 3
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 4
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 1
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          sS_rlc_Info:
          {
            sS_ul_RLC_Mode:
            [
              dl_UM_RLC_Mode: NULL
            ],
            sS_dl_RLC_Mode:
            {
              dl_PayloadSize: 136,
              dl_RLCModeInfo:
              [
                ul_UM_RLC_Mode:
                {
                  transmissionRLC_Discard:
                  [
                    timerBasedNoExplicit: dt100
                  ]
                }
              ]
            }
          },
          rB_LogCH_Mapping:
          {
            uLlogicalChannelIdentity: 1,
            dLlogicalChannelIdentity: 1,
            logicalChannelType: OMIT,
            cn_DomainIdentity: OMIT
          }
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 2
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          sS_rlc_Info:
          {
            sS_ul_RLC_Mode:
            [
              dl_AM_RLC_Mode:
              {
                inSequenceDelivery: GcTRUE,
                receivingWindowSize: rw32,
                dl_RLC_StatusInfo:
                {
                  timerStatusProhibit: tsp200,
                  timerEPC: OMIT,
                  missingPDU_Indicator: GcTRUE,
                  timerStatusPeriodic: OMIT
                }
              }
            ],
            sS_dl_RLC_Mode:
            {
              dl_PayloadSize: 128,
              dl_RLCModeInfo:
              [
                ul_AM_RLC_Mode:
                {
                  transmissionRLC_Discard:
                  [
                    noDiscard: dat15
                  ],
                  transmissionWindowSize: tw32,
                  timerRST: tr500,
                  max_RST: rst1,
                  pollingInfo:
                  {
                    timerPollProhibit: tpp200,
                    timerPoll: tp200,
                    poll_PDU: OMIT,
                    poll_SDU: sdu1,
                    lastTransmissionPDU_Poll: GcTRUE,
                    lastRetransmissionPDU_Poll: GcTRUE,
                    pollWindow: pw99,
                    timerPollPeriodic: OMIT
                  }
                }
              ]
            }
          },
          rB_LogCH_Mapping:
          {
            uLlogicalChannelIdentity: 2,
            dLlogicalChannelIdentity: 2,
            logicalChannelType: OMIT,
            cn_DomainIdentity: OMIT
          }
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 3
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          sS_rlc_Info:
          {
            sS_ul_RLC_Mode:
            [
              dl_AM_RLC_Mode:
              {
                inSequenceDelivery: GcTRUE,
                receivingWindowSize: rw32,
                dl_RLC_StatusInfo:
                {
                  timerStatusProhibit: tsp200,
                  timerEPC: OMIT,
                  missingPDU_Indicator: GcTRUE,
                  timerStatusPeriodic: OMIT
                }
              }
            ],
            sS_dl_RLC_Mode:
            {
              dl_PayloadSize: 128,
              dl_RLCModeInfo:
              [
                ul_AM_RLC_Mode:
                {
                  transmissionRLC_Discard:
                  [
                    noDiscard: dat15
                  ],
                  transmissionWindowSize: tw32,
                  timerRST: tr500,
                  max_RST: rst1,
                  pollingInfo:
                  {
                    timerPollProhibit: tpp200,
                    timerPoll: tp200,
                    poll_PDU: OMIT,
                    poll_SDU: sdu1,
                    lastTransmissionPDU_Poll: GcTRUE,
                    lastRetransmissionPDU_Poll: GcTRUE,
                    pollWindow: pw99,
                    timerPollPeriodic: OMIT
                  }
                }
              ]
            }
          },
          rB_LogCH_Mapping:
          {
            uLlogicalChannelIdentity: 3,
            dLlogicalChannelIdentity: 3,
            logicalChannelType: OMIT,
            cn_DomainIdentity: OMIT
          }
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 4
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          sS_rlc_Info:
          {
            sS_ul_RLC_Mode:
            [
              dl_AM_RLC_Mode:
              {
                inSequenceDelivery: GcTRUE,
                receivingWindowSize: rw32,
                dl_RLC_StatusInfo:
                {
                  timerStatusProhibit: tsp200,
                  timerEPC: OMIT,
                  missingPDU_Indicator: GcTRUE,
                  timerStatusPeriodic: OMIT
                }
              }
            ],
            sS_dl_RLC_Mode:
            {
              dl_PayloadSize: 128,
              dl_RLCModeInfo:
              [
                ul_AM_RLC_Mode:
                {
                  transmissionRLC_Discard:
                  [
                    noDiscard: dat15
                  ],
                  transmissionWindowSize: tw32,
                  timerRST: tr500,
                  max_RST: rst1,
                  pollingInfo:
                  {
                    timerPollProhibit: tpp200,
                    timerPoll: tp200,
                    poll_PDU: OMIT,
                    poll_SDU: sdu1,
                    lastTransmissionPDU_Poll: GcTRUE,
                    lastRetransmissionPDU_Poll: GcTRUE,
                    pollWindow: pw99,
                    timerPollPeriodic: OMIT
                  }
                }
              ]
            }
          },
          rB_LogCH_Mapping:
          {
            uLlogicalChannelIdentity: 4,
            dLlogicalChannelIdentity: 4,
            logicalChannelType: OMIT,
            cn_DomainIdentity: OMIT
          }
        }
      ]
    }

TTCN PDU: AT_CmdReq

(To search, click here and then press Ctrl+F)

    {
      cmd: "AT+CGEQREQ=1,
      2,
      64,
      64,
    ,
    ,
      1,
      320,
      "1E4",
      "1E5",
      1,
    ,
      3<CR>",
      sMS_BlockMode: OMIT
    }

TTCN PDU: AT_CmdCnf

(To search, click here and then press Ctrl+F)

    {
      result: OMIT,
      resultString: "<CR><LF>OK<CR><LF>",
      sMS_BlockMode: OMIT
    }

TTCN PDU: AT_CmdReq

(To search, click here and then press Ctrl+F)

    {
      cmd: "AT+CGDCONT=1,
      "IP",
      "ABCDEF",
      "200.1.1.80",
      0,
      0<CR>",
      sMS_BlockMode: OMIT
    }

TTCN PDU: AT_CmdCnf

(To search, click here and then press Ctrl+F)

    {
      result: OMIT,
      resultString: "<CR><LF>OK<CR><LF>",
      sMS_BlockMode: OMIT
    }

TTCN PDU: RLC_TR_DATA_IND

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: 0
      ],
      tM_message:
      [
        uL_CCCH_Message: PDU:
        {
          integrityCheckInfo: OMIT,
          message:
          [
            rrcConnectionRequest:
            {
              initialUE_Identity:
              [
                tmsi_and_LAI:
                {
                  tmsi: '00010001001000100011001101000100'B,
                  lai:
                  {
                    plmn_Identity:
                    {
                      mcc:
                      [
                        0,
                        0,
                        1
                      ],
                      mnc:
                      [
                        0,
                        1
                      ]
                    },
                    lac: '0000000000000001'B
                  }
                }
              ],
              establishmentCause: originatingInteractiveCall,
              protocolErrorIndicator: noError,
              measuredResultsOnRACH: OMIT,
              v3d0NonCriticalExtensions: OMIT
            }
          ]
        }
      ]
    }

TTCN PDU: RLC_UM_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: 0
      ],
      uM_message:
      [
        dL_CCCH_Message: PDU:
        {
          integrityCheckInfo: OMIT,
          message:
          [
            rrcConnectionSetup:
            [
              r3:
              {
                rrcConnectionSetup_r3:
                {
                  initialUE_Identity:
                  [
                    tmsi_and_LAI:
                    {
                      tmsi: '00010001001000100011001101000100'B,
                      lai:
                      {
                        plmn_Identity:
                        {
                          mcc:
                          [
                            0,
                            0,
                            1
                          ],
                          mnc:
                          [
                            0,
                            1
                          ]
                        },
                        lac: '0000000000000001'B
                      }
                    }
                  ],
                  rrc_TransactionIdentifier: 0,
                  activationTime: OMIT,
                  new_U_RNTI:
                  {
                    srnc_Identity: '000000000001'B,
                    s_RNTI: '00000000000000000001'B
                  },
                  new_c_RNTI: OMIT,
                  rrc_StateIndicator: cell_DCH,
                  utran_DRX_CycleLengthCoeff: 9,
                  capabilityUpdateRequirement:
                  {
                    ue_RadioCapabilityFDDUpdateRequirement: GcTRUE,
                    ue_RadioCapabilityTDDUpdateRequirement: GcFALSE,
                    systemSpecificCapUpdateReqList:
                    [
                      gsm
                    ]
                  },
                  srb_InformationSetupList:
                  [
                    {
                      rb_Identity: OMIT,
                      rlc_InfoChoice:
                      [
                        rlc_Info:
                        {
                          ul_RLC_Mode:
                          [
                            ul_UM_RLC_Mode:
                            {
                              transmissionRLC_Discard: OMIT
                            }
                          ],
                          dl_RLC_Mode:
                          [
                            dl_UM_RLC_Mode: NULL
                          ]
                        }
                      ],
                      rb_MappingInfo:
                      [
                        {
                          ul_LogicalChannelMappings:
                          [
                            oneLogicalChannel:
                            {
                              ul_TransportChannelType:
                              [
                                dch: 5
                              ],
                              logicalChannelIdentity: 1,
                              rlc_SizeList:
                              [
                                configured: NULL
                              ],
                              mac_LogicalChannelPriority: 1
                            }
                          ],
                          dl_LogicalChannelMappingList:
                          [
                            {
                              dl_TransportChannelType:
                              [
                                dch: 10
                              ],
                              logicalChannelIdentity: 1
                            }
                          ]
                        },

                        {
                          ul_LogicalChannelMappings:
                          [
                            oneLogicalChannel:
                            {
                              ul_TransportChannelType:
                              [
                                rach: NULL
                              ],
                              logicalChannelIdentity: 1,
                              rlc_SizeList:
                              [
                                explicitList:
                                [
                                  {
                                    rlc_SizeIndex: 1
                                  }
                                ]
                              ],
                              mac_LogicalChannelPriority: 1
                            }
                          ],
                          dl_LogicalChannelMappingList:
                          [
                            {
                              dl_TransportChannelType:
                              [
                                fach: NULL
                              ],
                              logicalChannelIdentity: 1
                            }
                          ]
                        }
                      ]
                    },

                    {
                      rb_Identity: OMIT,
                      rlc_InfoChoice:
                      [
                        rlc_Info:
                        {
                          ul_RLC_Mode:
                          [
                            ul_AM_RLC_Mode:
                            {
                              transmissionRLC_Discard:
                              [
                                noDiscard: dat15
                              ],
                              transmissionWindowSize: tw32,
                              timerRST: tr500,
                              max_RST: rst1,
                              pollingInfo:
                              {
                                timerPollProhibit: tpp200,
                                timerPoll: tp200,
                                poll_PDU: OMIT,
                                poll_SDU: sdu1,
                                lastTransmissionPDU_Poll: GcTRUE,
                                lastRetransmissionPDU_Poll: GcTRUE,
                                pollWindow: pw99,
                                timerPollPeriodic: OMIT
                              }
                            }
                          ],
                          dl_RLC_Mode:
                          [
                            dl_AM_RLC_Mode:
                            {
                              inSequenceDelivery: GcTRUE,
                              receivingWindowSize: rw32,
                              dl_RLC_StatusInfo:
                              {
                                timerStatusProhibit: tsp200,
                                timerEPC: OMIT,
                                missingPDU_Indicator: GcTRUE,
                                timerStatusPeriodic: OMIT
                              }
                            }
                          ]
                        }
                      ],
                      rb_MappingInfo:
                      [
                        {
                          ul_LogicalChannelMappings:
                          [
                            oneLogicalChannel:
                            {
                              ul_TransportChannelType:
                              [
                                dch: 5
                              ],
                              logicalChannelIdentity: 2,
                              rlc_SizeList:
                              [
                                configured: NULL
                              ],
                              mac_LogicalChannelPriority: 2
                            }
                          ],
                          dl_LogicalChannelMappingList:
                          [
                            {
                              dl_TransportChannelType:
                              [
                                dch: 10
                              ],
                              logicalChannelIdentity: 2
                            }
                          ]
                        },

                        {
                          ul_LogicalChannelMappings:
                          [
                            oneLogicalChannel:
                            {
                              ul_TransportChannelType:
                              [
                                rach: NULL
                              ],
                              logicalChannelIdentity: 2,
                              rlc_SizeList:
                              [
                                explicitList:
                                [
                                  {
                                    rlc_SizeIndex: 1
                                  }
                                ]
                              ],
                              mac_LogicalChannelPriority: 2
                            }
                          ],
                          dl_LogicalChannelMappingList:
                          [
                            {
                              dl_TransportChannelType:
                              [
                                fach: NULL
                              ],
                              logicalChannelIdentity: 2
                            }
                          ]
                        }
                      ]
                    },

                    {
                      rb_Identity: OMIT,
                      rlc_InfoChoice:
                      [
                        rlc_Info:
                        {
                          ul_RLC_Mode:
                          [
                            ul_AM_RLC_Mode:
                            {
                              transmissionRLC_Discard:
                              [
                                noDiscard: dat15
                              ],
                              transmissionWindowSize: tw32,
                              timerRST: tr500,
                              max_RST: rst1,
                              pollingInfo:
                              {
                                timerPollProhibit: tpp200,
                                timerPoll: tp200,
                                poll_PDU: OMIT,
                                poll_SDU: sdu1,
                                lastTransmissionPDU_Poll: GcTRUE,
                                lastRetransmissionPDU_Poll: GcTRUE,
                                pollWindow: pw99,
                                timerPollPeriodic: OMIT
                              }
                            }
                          ],
                          dl_RLC_Mode:
                          [
                            dl_AM_RLC_Mode:
                            {
                              inSequenceDelivery: GcTRUE,
                              receivingWindowSize: rw32,
                              dl_RLC_StatusInfo:
                              {
                                timerStatusProhibit: tsp200,
                                timerEPC: OMIT,
                                missingPDU_Indicator: GcTRUE,
                                timerStatusPeriodic: OMIT
                              }
                            }
                          ]
                        }
                      ],
                      rb_MappingInfo:
                      [
                        {
                          ul_LogicalChannelMappings:
                          [
                            oneLogicalChannel:
                            {
                              ul_TransportChannelType:
                              [
                                dch: 5
                              ],
                              logicalChannelIdentity: 3,
                              rlc_SizeList:
                              [
                                configured: NULL
                              ],
                              mac_LogicalChannelPriority: 3
                            }
                          ],
                          dl_LogicalChannelMappingList:
                          [
                            {
                              dl_TransportChannelType:
                              [
                                dch: 10
                              ],
                              logicalChannelIdentity: 3
                            }
                          ]
                        },

                        {
                          ul_LogicalChannelMappings:
                          [
                            oneLogicalChannel:
                            {
                              ul_TransportChannelType:
                              [
                                rach: NULL
                              ],
                              logicalChannelIdentity: 3,
                              rlc_SizeList:
                              [
                                explicitList:
                                [
                                  {
                                    rlc_SizeIndex: 1
                                  }
                                ]
                              ],
                              mac_LogicalChannelPriority: 3
                            }
                          ],
                          dl_LogicalChannelMappingList:
                          [
                            {
                              dl_TransportChannelType:
                              [
                                fach: NULL
                              ],
                              logicalChannelIdentity: 3
                            }
                          ]
                        }
                      ]
                    },

                    {
                      rb_Identity: OMIT,
                      rlc_InfoChoice:
                      [
                        rlc_Info:
                        {
                          ul_RLC_Mode:
                          [
                            ul_AM_RLC_Mode:
                            {
                              transmissionRLC_Discard:
                              [
                                noDiscard: dat15
                              ],
                              transmissionWindowSize: tw32,
                              timerRST: tr500,
                              max_RST: rst1,
                              pollingInfo:
                              {
                                timerPollProhibit: tpp200,
                                timerPoll: tp200,
                                poll_PDU: OMIT,
                                poll_SDU: sdu1,
                                lastTransmissionPDU_Poll: GcTRUE,
                                lastRetransmissionPDU_Poll: GcTRUE,
                                pollWindow: pw99,
                                timerPollPeriodic: OMIT
                              }
                            }
                          ],
                          dl_RLC_Mode:
                          [
                            dl_AM_RLC_Mode:
                            {
                              inSequenceDelivery: GcTRUE,
                              receivingWindowSize: rw32,
                              dl_RLC_StatusInfo:
                              {
                                timerStatusProhibit: tsp200,
                                timerEPC: OMIT,
                                missingPDU_Indicator: GcTRUE,
                                timerStatusPeriodic: OMIT
                              }
                            }
                          ]
                        }
                      ],
                      rb_MappingInfo:
                      [
                        {
                          ul_LogicalChannelMappings:
                          [
                            oneLogicalChannel:
                            {
                              ul_TransportChannelType:
                              [
                                dch: 5
                              ],
                              logicalChannelIdentity: 4,
                              rlc_SizeList:
                              [
                                configured: NULL
                              ],
                              mac_LogicalChannelPriority: 4
                            }
                          ],
                          dl_LogicalChannelMappingList:
                          [
                            {
                              dl_TransportChannelType:
                              [
                                dch: 10
                              ],
                              logicalChannelIdentity: 4
                            }
                          ]
                        },

                        {
                          ul_LogicalChannelMappings:
                          [
                            oneLogicalChannel:
                            {
                              ul_TransportChannelType:
                              [
                                rach: NULL
                              ],
                              logicalChannelIdentity: 4,
                              rlc_SizeList:
                              [
                                explicitList:
                                [
                                  {
                                    rlc_SizeIndex: 1
                                  }
                                ]
                              ],
                              mac_LogicalChannelPriority: 4
                            }
                          ],
                          dl_LogicalChannelMappingList:
                          [
                            {
                              dl_TransportChannelType:
                              [
                                fach: NULL
                              ],
                              logicalChannelIdentity: 4
                            }
                          ]
                        }
                      ]
                    }
                  ],
                  ul_CommonTransChInfo:
                  {
                    tfc_Subset: OMIT,
                    prach_TFCS: OMIT,
                    modeSpecificInfo:
                    [
                      fdd:
                      {
                        ul_TFCS:
                        [
                          normalTFCI_Signalling:
                          [
                            complete:
                            {
                              ctfcSize:
                              [
                                ctfc2Bit:
                                [
                                  {
                                    ctfc2: 0,
                                    powerOffsetInformation:
                                    {
                                      gainFactorInformation:
                                      [
                                        computedGainFactors: 0
                                      ],
                                      powerOffsetPp_m: OMIT
                                    }
                                  },

                                  {
                                    ctfc2: 1,
                                    powerOffsetInformation:
                                    {
                                      gainFactorInformation:
                                      [
                                        signalledGainFactors:
                                        {
                                          modeSpecificInfo:
                                          [
                                            fdd:
                                            {
                                              gainFactorBetaC: 11
                                            }
                                          ],
                                          gainFactorBetaD: 15,
                                          referenceTFC_ID: 0
                                        }
                                      ],
                                      powerOffsetPp_m: OMIT
                                    }
                                  }
                                ]
                              ]
                            }
                          ]
                        ]
                      }
                    ]
                  },
                  ul_AddReconfTransChInfoList:
                  [
                    {
                      ul_TransportChannelType: dch,
                      transportChannelIdentity: 5,
                      transportFormatSet:
                      [
                        dedicatedTransChTFS:
                        {
                          tti:
                          [
                            tti10:
                            [
                              {
                                rlc_Size:
                                [
                                  bitMode:
                                  [
                                    sizeType2:
                                    {
                                      part1: 2,
                                      part2: OMIT
                                    }
                                  ]
                                ],
                                numberOfTbSizeList:
                                [
                                  [
                                    zero: NULL
                                  ],

                                  [
                                    one: NULL
                                  ]
                                ],
                                logicalChannelList:
                                [
                                  allSizes: NULL
                                ]
                              }
                            ]
                          ],
                          semistaticTF_Information:
                          {
                            channelCodingType:
                            [
                              convolutional: third
                            ],
                            rateMatchingAttribute# 192 # crc_Size# crc16
                          }
                        }
                      ]
                    }
                  ]
                  # dl_CommonTransChInfo#
                  {
                    sccpch_TFCS# OMIT# modeSpecificInfo#
                    [
                      fdd#
                      {
                        dl_Parameters#
                        [
                          sameAsUL# NULL
                        ]
                      }
                    ]
                  }
                  # dl_AddReconfTransChInfoList#
                  [
                    {
                      dl_TransportChannelType# dch# dl_transportChannelIdentity# 10 # tfs_SignallingMode#
                      [
                        sameAsULTrCH#
                        {
                          ul_TransportChannelType# dch# ul_TransportChannelIdentity# 5
                        }
                      ]
                      # dch_QualityTarget#
                      {
                        bler_QualityValue# #20
                      }
                      # dummy# OMIT
                    }
                  ]
                  # frequencyInfo# OMIT# maxAllowedUL_TX_Power# OMIT# ul_ChannelRequirement#
                  [
                    ul_DPCH_Info#
                    {
                      ul_DPCH_PowerControlInfo#
                      [
                        fdd#
                        {
                          dpcch_PowerOffset# #40 # pc_Preamble# 1 # sRB_delay# 7 # powerControlAlgorithm#
                          [
                            algorithm1# 1
                          ]
                        }
                      ]
                      # modeSpecificInfo#
                      [
                        fdd#
                        {
                          scramblingCodeType# longSC# scramblingCode# 0 # numberOfDPDCH# OMIT# spreadingFactor# sf64# tfci_Existence# GcTRUE # numberOfFBI_Bits# OMIT# puncturingLimit# pl1
                        }
                      ]
                    }
                  ]
                  # dl_CommonInformation#
                  {
                    dl_DPCH_InfoCommon#
                    {
                      cfnHandling#
                      [
                        initialise#
                        {
                          cfntargetsfnframeoffset# OMIT
                        }
                      ]
                      # modeSpecificInfo#
                      [
                        fdd#
                        {
                          dl_DPCH_PowerControlInfo#
                          {
                            modeSpecificInfo#
                            [
                              fdd#
                              {
                                dpc_Mode# singleTPC
                              }
                            ]
                          }
                          # powerOffsetPilot_pdpdch# 0 # dl_rate_matching_restriction# OMIT# spreadingFactorAndPilot#
                          [
                            sfd128# pb4
                          ]
                          # positionFixedOrFlexible# fixed# tfci_Existence# GcFALSE
                        }
                      ]
                    }
                    # modeSpecificInfo#
                    [
                      fdd#
                      {
                        defaultDPCH_OffsetValue# 0 # dpch_CompressedModeInfo# OMIT# tx_DiversityMode# noDiversity# ssdt_Information# OMIT
                      }
                    ]
                  }
                  # dl_InformationPerRL_List#
                  [
                    {
                      modeSpecificInfo#
                      [
                        fdd#
                        {
                          primaryCPICH_Info#
                          {
                            primaryScramblingCode# 100
                          }
                          # pdsch_SHO_DCH_Info# OMIT# pdsch_CodeMapping# OMIT
                        }
                      ]
                      # dl_DPCH_InfoPerRL#
                      [
                        fdd#
                        {
                          pCPICH_UsageForChannelEst# mayBeUsed# dpch_FrameOffset# 0 # secondaryCPICH_Info# OMIT# dl_ChannelisationCodeList#
                          [
                            {
                              secondaryScramblingCode# 1 # sf_AndCodeNumber#
                              [
                                sf128# 0
                              ]
                              # scramblingCodeChange# noCodeChange
                            }
                          ]
                          # tpc_CombinationIndex# 0 # ssdt_CellIdentity# OMIT# closedLoopTimingAdjMode# OMIT
                        }
                      ]
                      # sccpch_InfoforFACH# OMIT
                    }
                  ]
                }
                # laterNonCriticalExtensions# OMIT
              }
            ]
          ]
        }
      ]
      # specialLI# GcTRUE
    }

TTCN PDU: RLC_AM_DATA_IND

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 2
      ],
      integrityResult:
      [
        integrityUsed: i_pass
      ],
      aM_message:
      [
        uL_DCCH_Message: PDU:
        {
          integrityCheckInfo: OMIT,
          message:
          [
            rrcConnectionSetupComplete:
            {
              rrc_TransactionIdentifier: 0,
              startList:
              [
                {
                  cn_DomainIdentity: ps_domain,
                  start_Value: '00000000000000000010'B
                },

                {
                  cn_DomainIdentity: cs_domain,
                  start_Value: '00000000000000000010'B
                }
              ],
              ue_RadioAccessCapability:
              {
                accessStratumReleaseIndicator: r99,
                pdcp_Capability:
                {
                  losslessSRNS_RelocationSupport: GcTRUE,
                  supportForRfc2507:
                  [
                    supported: by8192
                  ]
                },
                rlc_Capability:
                {
                  totalRLC_AM_BufferSize: kb50,
                  maximumRLC_WindowSize: mws2047,
                  maximumAM_EntityNumber: am6
                },
                transportChannelCapability:
                {
                  dl_TransChCapability:
                  {
                    maxNoBitsReceived: b5120,
                    maxConvCodeBitsReceived: b1280,
                    turboDecodingSupport:
                    [
                      supported: b5120
                    ],
                    maxSimultaneousTransChs: e8,
                    maxSimultaneousCCTrCH_Count: 1,
                    maxReceivedTransportBlocks: tb16,
                    maxNumberOfTFC: tfc96,
                    maxNumberOfTF: tf64
                  },
                  ul_TransChCapability:
                  {
                    maxNoBitsTransmitted: b3840,
                    maxConvCodeBitsTransmitted: b1280,
                    turboEncodingSupport:
                    [
                      supported: b3840
                    ],
                    maxSimultaneousTransChs: e8,
                    modeSpecificInfo:
                    [
                      fdd: NULL
                    ],
                    maxTransmittedBlocks: tb8,
                    maxNumberOfTFC: tfc32,
                    maxNumberOfTF: tf32
                  }
                },
                rf_Capability:
                {
                  fddRF_Capability:
                  {
                    ue_PowerClass: 4,
                    txRxFrequencySeparation: mhz190
                  },
                  tddRF_Capability: OMIT
                },
                physicalChannelCapability:
                {
                  fddPhysChCapability:
                  {
                    downlinkPhysChCapability:
                    {
                      maxNoDPCH_PDSCH_Codes: 3,
                      maxNoPhysChBitsReceived: b9600,
                      supportForSF_512: GcFALSE,
                      supportOfPDSCH: GcFALSE,
                      simultaneousSCCPCH_DPCH_Reception:
                      [
                        notSupported: NULL
                      ]
                    },
                    uplinkPhysChCapability:
                    {
                      maxNoDPDCH_BitsTransmitted: b2400,
                      supportOfPCPCH: GcFALSE
                    }
                  },
                  tddPhysChCapability: OMIT
                },
                ue_MultiModeRAT_Capability:
                {
                  multiRAT_CapabilityList:
                  {
                    supportOfGSM: GcFALSE,
                    supportOfMulticarrier: GcFALSE
                  },
                  multiModeCapability: fdd
                },
                securityCapability:
                {
                  cipheringAlgorithmCap: '0000000000000001'B,
                  integrityProtectionAlgorithmCap: '0000000000000010'B
                },
                ue_positioning_Capability:
                {
                  standaloneLocMethodsSupported: GcFALSE,
                  ue_BasedOTDOA_Supported: GcFALSE,
                  networkAssistedGPS_Supported: noNetworkAssistedGPS,
                  supportForUE_GPS_TimingOfCellFrames: GcFALSE,
                  supportForIPDL: GcFALSE
                },
                measurementCapability:
                {
                  downlinkCompressedMode:
                  {
                    fdd_Measurements: GcTRUE,
                    tdd_Measurements: OMIT,
                    gsm_Measurements:
                    {
                      gsm900: GcTRUE,
                      dcs1800: GcTRUE,
                      gsm1900: GcFALSE
                    },
                    multiCarrierMeasurements: GcFALSE
                  },
                  uplinkCompressedMode:
                  {
                    fdd_Measurements: GcTRUE,
                    tdd_Measurements: OMIT,
                    gsm_Measurements:
                    {
                      gsm900: GcTRUE,
                      dcs1800: GcTRUE,
                      gsm1900: GcFALSE
                    },
                    multiCarrierMeasurements: GcFALSE
                  }
                }
              },
              ue_RATSpecificCapability: OMIT,
              v370NonCriticalExtensions: OMIT
            }
          ]
        }
      ]
    }

TTCN PDU: RRC_DataInd

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      rB_Id: 3,
      ch: OMIT,
      sapId: OMIT,
      cN_Domain: 1,
      start: '00000000000000000010'B,
      msg: PDU:
      {
        skipIndicator: '0000'B,
        gMMProtocolDiscriminator: '1000'B,
        msgType: '00001100'B,
        serviceType:
        {
          spare1: '0'B,
          type: '000'B
        },
        ciphKeySeqNo:
        {
          spare1: '0'B,
          keySeq: '000'B
        },
        ptmsi:
        {
          iel: '05'O,
          iDigit1: '1111'B,
          oddEvenInd: '0'B,
          typeOfId: '100'B,
          otherDigits: '12345678'O
        },
        pDP_ContextStatus:
        {
          iei: '00110010'B,
          iel: '02'O,
          nSAPI: '0000000000000000'B
        }
      }
    }

TTCN PDU: RRC_DataReq

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      rB_Id: 3,
      ch: OMIT,
      sapId: OMIT,
      cN_Domain: 1,
      msg: PDU:
      {
        skipIndicator: '0000'B,
        gMMProtocolDiscriminator: '1000'B,
        msgType: '00010010'B,
        imeisvReq:
        {
          spare1: '0'B,
          value: '000'B
        },
        ciphAlgorithm:
        {
          spare1: '0'B,
          algorithm: '001'B
        },
        acRefNo:
        {
          value: '0011'B
        },
        forceToStandby:
        {
          spare: '0'B,
          value: '000'B
        },
        authRand:
        {
          iei: '00100001'B,
          randValue: '01010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101'B
        },
        gprsCiphKeySeqNo:
        {
          iei: '1000'B,
          spare1: '0'B,
          keySeq: '001'B
        },
        aUTN:
        {
          iei: '00101000'B,
          iel: '10'O,
          aUTN: '01100110000100010000000000110011001000101101110100000000000000000101010101000100011101110110011000010001000000000011001100100010'B
        }
      }
    }

TTCN PDU: Assignment:[3] tcv_TmpAuthAndCiphRs

(To search, click here and then press Ctrl+F)

    := PDU:
    {
      skipIndicator: '0000'B,
      gMMProtocolDiscriminator: '1000'B,
      msgType: '00010011'B,
      spare4: '0000'B,
      acRefNo:
      {
        value: '0011'B
      },
      authRsp:
      {
        iei: '00100010'B,
        value: '01010101010001000111011101100110'B
      },
      imeisv: OMIT,
      authRspExt:
      {
        iei: '00101001'B,
        iel: '0C'O,
        rES: '000100010000000000110011001000101101110111001100111111111110111010011001100010001011101110101010'B
      }
    }

TTCN PDU: RRC_DataInd

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      rB_Id: 3,
      ch: OMIT,
      sapId: OMIT,
      cN_Domain: 1,
      start: OMIT,
      msg: PDU:
      {
        skipIndicator: '0000'B,
        gMMProtocolDiscriminator: '1000'B,
        msgType: '00010011'B,
        spare4: '0000'B,
        acRefNo:
        {
          value: '0011'B
        },
        authRsp:
        {
          iei: '00100010'B,
          value: '01010101010001000111011101100110'B
        },
        imeisv: OMIT,
        authRspExt:
        {
          iei: '00101001'B,
          iel: '0C'O,
          rES: '000100010000000000110011001000101101110111001100111111111110111010011001100010001011101110101010'B
        }
      }
    }

TTCN PDU: CRLC_SecurityMode_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      rlcSecurityInfo:
      {
        cn_DomainIdentity: ps_domain,
        startValue: '00000000000000000000'B,
        cipheringKey: OMIT,
        integrityKey: '01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100'B,
        gsmCipheringKey: OMIT
      }
    }

TTCN PDU: CRLC_SetRRC_MessageSN_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: 0
      ],
      count_I_LSB_UL: OMIT,
      count_I_LSB_DL: 0
    }

TTCN PDU: CRLC_SetRRC_MessageSN_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 1
      ],
      count_I_LSB_UL: OMIT,
      count_I_LSB_DL: 0
    }

TTCN PDU: CRLC_SetRRC_MessageSN_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 2
      ],
      count_I_LSB_UL: OMIT,
      count_I_LSB_DL: 0
    }

TTCN PDU: CRLC_SetRRC_MessageSN_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 3
      ],
      count_I_LSB_UL: OMIT,
      count_I_LSB_DL: 0
    }

TTCN PDU: CRLC_SetRRC_MessageSN_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 4
      ],
      count_I_LSB_UL: OMIT,
      count_I_LSB_DL: 0
    }

TTCN PDU: CRLC_Integrity_Activate_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      cn_DomainIdentity: ps_domain,
      integrityActivationInfo:
      [
        integrityProtectionModeInfo:
        {
          integrityProtectionModeCommand:
          [
            startIntegrityProtection:
            {
              integrityProtInitNumber: '00001111000011110000111100001111'B
            }
          ],
          integrityProtectionAlgorithm: uia1
        }
      ]
    }

TTCN PDU: CRLC_Integrity_Activate_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      cn_DomainIdentity: ps_domain,
      integrityActivationInfo:
      [
        ul_IntegProtActivationInfo:
        [
          {
            rb_Identity: 2,
            rrc_MessageSequenceNumber: 0
          }
        ]
      ]
    }

TTCN PDU: RLC_AM_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 2
      ],
      confirmationRequest:
      [
        noConfirmationRequest: NULL
      ],
      aM_message:
      [
        dL_DCCH_Message: PDU:
        {
          integrityCheckInfo:
          {
            messageAuthenticationCode: '00101001110000010111010101011011'B,
            rrc_MessageSequenceNumber: 1
          },
          message:
          [
            securityModeCommand:
            [
              r3:
              {
                securityModeCommand_r3:
                {
                  rrc_TransactionIdentifier: 0,
                  securityCapability:
                  {
                    cipheringAlgorithmCap: '0000000000000001'B,
                    integrityProtectionAlgorithmCap: '0000000000000010'B
                  },
                  cipheringModeInfo: OMIT,
                  integrityProtectionModeInfo:
                  {
                    integrityProtectionModeCommand:
                    [
                      startIntegrityProtection:
                      {
                        integrityProtInitNumber: '00001111000011110000111100001111'B
                      }
                    ],
                    integrityProtectionAlgorithm: uia1
                  },
                  cn_DomainIdentity: ps_domain,
                  ue_SystemSpecificSecurityCap: OMIT
                },
                laterNonCriticalExtensions: OMIT
              }
            ]
          ]
        }
      ]
    }

TTCN PDU: RLC_AM_DATA_IND

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 2
      ],
      integrityResult:
      [
        integrityUsed: i_pass
      ],
      aM_message:
      [
        uL_DCCH_Message: PDU:
        {
          integrityCheckInfo:
          {
            messageAuthenticationCode: '10001011001000110111110011100010'B,
            rrc_MessageSequenceNumber: 1
          },
          message:
          [
            securityModeComplete:
            {
              rrc_TransactionIdentifier: 0,
              ul_IntegProtActivationInfo:
              {
                rrc_MessageSequenceNumberList:
                [
                  0,
                  0,
                  0,
                  0,
                  0
                ]
              },
              rb_UL_CiphActivationTimeInfo: OMIT,
              laterNonCriticalExtensions: OMIT
            }
          ]
        }
      ]
    }

TTCN PDU: CRLC_Integrity_Activate_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      cn_DomainIdentity: ps_domain,
      integrityActivationInfo:
      [
        ul_IntegProtActivationInfo:
        [
          {
            rb_Identity: 0,
            rrc_MessageSequenceNumber: 0
          },

          {
            rb_Identity: 1,
            rrc_MessageSequenceNumber: 0
          },

          {
            rb_Identity: 3,
            rrc_MessageSequenceNumber: 0
          },

          {
            rb_Identity: 4,
            rrc_MessageSequenceNumber: 0
          }
        ]
      ]
    }

TTCN PDU: Assignment:[17] tcv_ActPDP_ContextReq :

(To search, click here and then press Ctrl+F)

    {
      ti:
      {
        tiFlag: '0'B,
        tiVal: '000'B
      },
      sM_ProtocolDiscriminator: '1010'B,
      msgType: '01000001'B,
      requestedNSAPI:
      {
        spare: '0000'B,
        nSAPI_Value: '0101'B
      },
      requestedLLC_SAPI:
      {
        spare: '0000'B,
        nSAPI_Value: '0011'B
      },
      requestedQoS:
      {
        length: '0B'O,
        spare: '00'B,
        dlyClass: '011'B,
        relabilityClass: '011'B,
        peakThroughput: '0100'B,
        spare1: '0'B,
        precedenceClass: '000'B,
        spare2: '000'B,
        meanThroughput: '11111'B,
        trafficClass: '011'B,
        deliveryOrder: '01'B,
        deliveryErrorSDU: '010'B,
        maxSDUSize: '20'O,
        maxBitRateUplink: '40'O,
        maxBitRateDnlink: '40'O,
        residualBER: '0111'B,
        sduErrRatio: '0100'B,
        transDly: '000000'B,
        trafficHandpro: '11'B,
        bitRateUplink: '00'O,
        bitRateDnlink: '00'O
      },
      pDP_Address:
      {
        length: '06'O,
        spare: '0000'B,
        pDP_TypeOrg: '0001'B,
        pDP_TypeNo: '21'O,
        addrInfo: 'C8010150'O
      },
      accessPtName:
      {
        iei: '00101000'B,
        length: '07'O,
        accessPtName: '06414243444546'O
      },
      protocolConfOpts: OMIT
    }

TTCN PDU: RRC_DataInd

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      rB_Id: 3,
      ch: OMIT,
      sapId: OMIT,
      cN_Domain: 1,
      start: OMIT,
      msg: PDU:
      {
        ti:
        {
          tiFlag: '0'B,
          tiVal: '000'B
        },
        sM_ProtocolDiscriminator: '1010'B,
        msgType: '01000001'B,
        requestedNSAPI:
        {
          spare: '0000'B,
          nSAPI_Value: '0101'B
        },
        requestedLLC_SAPI:
        {
          spare: '0000'B,
          nSAPI_Value: '0011'B
        },
        requestedQoS:
        {
          length: '0B'O,
          spare: '00'B,
          dlyClass: '011'B,
          relabilityClass: '011'B,
          peakThroughput: '0100'B,
          spare1: '0'B,
          precedenceClass: '000'B,
          spare2: '000'B,
          meanThroughput: '11111'B,
          trafficClass: '011'B,
          deliveryOrder: '01'B,
          deliveryErrorSDU: '010'B,
          maxSDUSize: '20'O,
          maxBitRateUplink: '40'O,
          maxBitRateDnlink: '40'O,
          residualBER: '0111'B,
          sduErrRatio: '0100'B,
          transDly: '000000'B,
          trafficHandpro: '11'B,
          bitRateUplink: '00'O,
          bitRateDnlink: '00'O
        },
        pDP_Address:
        {
          length: '06'O,
          spare: '0000'B,
          pDP_TypeOrg: '0001'B,
          pDP_TypeNo: '21'O,
          addrInfo: 'C8010150'O
        },
        accessPtName:
        {
          iei: '00101000'B,
          length: '07'O,
          accessPtName: '06414243444546'O
        },
        protocolConfOpts: OMIT
      }
    }

TTCN PDU: CPHY_Frame_Number_CNF

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 26
      ],
      frameNumber: 114
    }

TTCN PDU: RLC_AM_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 2
      ],
      confirmationRequest:
      [
        confirmationRequested: 0
      ],
      aM_message:
      [
        dL_DCCH_Message: PDU:
        {
          integrityCheckInfo:
          {
            messageAuthenticationCode: '00101100101001101110001111000110'B,
            rrc_MessageSequenceNumber: 2
          },
          message:
          [
            radioBearerSetup:
            [
              r3:
              {
                radioBearerSetup_r3:
                {
                  rrc_TransactionIdentifier: 0,
                  integrityProtectionModeInfo: OMIT,
                  cipheringModeInfo: OMIT,
                  activationTime: 104,
                  new_U_RNTI: OMIT,
                  new_C_RNTI: OMIT,
                  rrc_StateIndicator: cell_DCH,
                  utran_DRX_CycleLengthCoeff: OMIT,
                  ura_Identity: OMIT,
                  cn_InformationInfo: OMIT,
                  srb_InformationSetupList: OMIT,
                  rab_InformationSetupList:
                  [
                    {
                      rab_Info:
                      {
                        rab_Identity:
                        [
                          gsm_MAP_RAB_Identity: '00000101'B
                        ],
                        cn_DomainIdentity: ps_domain,
                        nas_Synchronisation_Indicator: OMIT,
                        re_EstablishmentTimer: useT315
                      },
                      rb_InformationSetupList:
                      [
                        {
                          rb_Identity: 20,
                          pdcp_Info:
                          {
                            losslessSRNS_RelocSupport:
                            [
                              notSupported: NULL
                            ],
                            pdcp_PDU_Header: absent,
                            headerCompressionInfoList: OMIT
                          },
                          rlc_InfoChoice:
                          [
                            rlc_Info:
                            {
                              ul_RLC_Mode:
                              [
                                ul_AM_RLC_Mode:
                                {
                                  transmissionRLC_Discard:
                                  [
                                    noDiscard: dat15
                                  ],
                                  transmissionWindowSize: tw128,
                                  timerRST: tr500,
                                  max_RST: rst4,
                                  pollingInfo:
                                  {
                                    timerPollProhibit: tpp200,
                                    timerPoll: tp200,
                                    poll_PDU: OMIT,
                                    poll_SDU: sdu1,
                                    lastTransmissionPDU_Poll: GcTRUE,
                                    lastRetransmissionPDU_Poll: GcTRUE,
                                    pollWindow: pw99,
                                    timerPollPeriodic: OMIT
                                  }
                                }
                              ],
                              dl_RLC_Mode:
                              [
                                dl_AM_RLC_Mode:
                                {
                                  inSequenceDelivery: GcTRUE,
                                  receivingWindowSize: rw128,
                                  dl_RLC_StatusInfo:
                                  {
                                    timerStatusProhibit: tsp200,
                                    timerEPC: OMIT,
                                    missingPDU_Indicator: GcTRUE,
                                    timerStatusPeriodic: OMIT
                                  }
                                }
                              ]
                            }
                          ],
                          rb_MappingInfo:
                          [
                            {
                              ul_LogicalChannelMappings:
                              [
                                oneLogicalChannel:
                                {
                                  ul_TransportChannelType:
                                  [
                                    dch: 1
                                  ],
                                  logicalChannelIdentity: OMIT,
                                  rlc_SizeList:
                                  [
                                    configured: NULL
                                  ],
                                  mac_LogicalChannelPriority: 8
                                }
                              ],
                              dl_LogicalChannelMappingList:
                              [
                                {
                                  dl_TransportChannelType:
                                  [
                                    dch: 6
                                  ],
                                  logicalChannelIdentity: OMIT
                                }
                              ]
                            },

                            {
                              ul_LogicalChannelMappings:
                              [
                                oneLogicalChannel:
                                {
                                  ul_TransportChannelType:
                                  [
                                    rach: NULL
                                  ],
                                  logicalChannelIdentity: 7,
                                  rlc_SizeList:
                                  [
                                    explicitList:
                                    [
                                      {
                                        rlc_SizeIndex: 2
                                      }
                                    ]
                                  ],
                                  mac_LogicalChannelPriority: 8
                                }
                              ],
                              dl_LogicalChannelMappingList:
                              [
                                {
                                  dl_TransportChannelType:
                                  [
                                    fach: NULL
                                  ],
                                  logicalChannelIdentity: 7
                                }
                              ]
                            }
                          ]
                        }
                      ]
                    }
                  ],
                  rb_InformationAffectedList: OMIT,
                  dl_CounterSynchronisationInfo: OMIT,
                  ul_CommonTransChInfo:
                  {
                    tfc_Subset: OMIT,
                    prach_TFCS: OMIT,
                    modeSpecificInfo:
                    [
                      fdd:
                      {
                        ul_TFCS:
                        [
                          normalTFCI_Signalling:
                          [
                            complete:
                            {
                              ctfcSize:
                              [
                                ctfc4Bit:
                                [
                                  {
                                    ctfc4: 0,
                                    powerOffsetInformation:
                                    {
                                      gainFactorInformation:
                                      [
                                        computedGainFactors: 0
                                      ],
                                      powerOffsetPp_m: OMIT
                                    }
                                  },

                                  {
                                    ctfc4: 1,
                                    powerOffsetInformation:
                                    {
                                      gainFactorInformation:
                                      [
                                        computedGainFactors: 0
                                      ],
                                      powerOffsetPp_m: OMIT
                                    }
                                  },

                                  {
                                    ctfc4: 2,
                                    powerOffsetInformation:
                                    {
                                      gainFactorInformation:
                                      [
                                        computedGainFactors: 0
                                      ],
                                      powerOffsetPp_m: OMIT
                                    }
                                  },

                                  {
                                    ctfc4: 3,
                                    powerOffsetInformation:
                                    {
                                      gainFactorInformation:
                                      [
                                        computedGainFactors: 0
                                      ],
                                      powerOffsetPp_m: OMIT
                                    }
                                  },

                                  {
                                    ctfc4: 4,
                                    powerOffsetInformation:
                                    {
                                      gainFactorInformation:
                                      [
                                        computedGainFactors: 0
                                      ],
                                      powerOffsetPp_m: OMIT
                                    }
                                  },

                                  {
                                    ctfc4: 5,
                                    powerOffsetInformation:
                                    {
                                      gainFactorInformation:
                                      [
                                        computedGainFactors: 0
                                      ],
                                      powerOffsetPp_m: OMIT
                                    }
                                  },

                                  {
                                    ctfc4: 6,
                                    powerOffsetInformation:
                                    {
                                      gainFactorInformation:
                                      [
                                        computedGainFactors: 0
                                      ],
                                      powerOffsetPp_m: OMIT
                                    }
                                  },

                                  {
                                    ctfc4: 7,
                                    powerOffsetInformation:
                                    {
                                      gainFactorInformation:
                                      [
                                        computedGainFactors: 0
                                      ],
                                      powerOffsetPp_m: OMIT
                                    }
                                  },

                                  {
                                    ctfc4: 8,
                                    powerOffsetInformation:
                                    {
                                      gainFactorInformation:
                                      [
                                        computedGainFactors: 0
                                      ],
                                      powerOffsetPp_m: OMIT
                                    }
                                  },

                                  {
                                    ctfc4: 9,
                                    powerOffsetInformation:
                                    {
                                      gainFactorInformation:
                                      [
                                        signalledGainFactors:
                                        {
                                          modeSpecificInfo:
                                          [
                                            fdd:
                                            {
                                              gainFactorBetaC: 9
                                            }
                                          ],
                                          gainFactorBetaD: 15,
                                          referenceTFC_ID: 0
                                        }
                                      ],
                                      powerOffsetPp_m: OMIT
                                    }
                                  }
                                ]
                              ]
                            }
                          ]
                        ]
                      }
                    ]
                  },
                  ul_deletedTransChInfoList: OMIT,
                  ul_AddReconfTransChInfoList:
                  [
                    {
                      ul_TransportChannelType: dch,
                      transportChannelIdentity: 1,
                      transportFormatSet:
                      [
                        dedicatedTransChTFS:
                        {
                          tti:
                          [
                            tti20:
                            [
                              {
                                rlc_Size:
                                [
                                  octetModeType1:
                                  [
                                    sizeType2:
                                    {
                                      part1: 2,
                                      part2: OMIT
                                    }
                                  ]
                                ],
                                numberOfTbSizeList:
                                [
                                  [
                                    zero: NULL
                                  ],

                                  [
                                    one: NULL
                                  ],

                                  [
                                    small: 2
                                  ],

                                  [
                                    small: 3
                                  ],

                                  [
                                    small: 4
                                  ]
                                ],
                                logicalChannelList:
                                [
                                  allSizes: NULL
                                ]
                              }
                            ]
                          ],
                          semistaticTF_Information:
                          {
                            channelCodingType:
                            [
                              turbo: NULL
                            ],
                            rateMatchingAttribute# 150 # crc_Size# crc16
                          }
                        }
                      ]
                    }
                    #
                    {
                      ul_TransportChannelType# dch# transportChannelIdentity# 5 # transportFormatSet#
                      [
                        dedicatedTransChTFS#
                        {
                          tti#
                          [
                            tti40#
                            [
                              {
                                rlc_Size#
                                [
                                  bitMode#
                                  [
                                    sizeType2#
                                    {
                                      part1# 2 # part2# OMIT
                                    }
                                  ]
                                ]
                                # numberOfTbSizeList#
                                [
                                  [
                                    zero# NULL
                                  ]
                                  #
                                  [
                                    one# NULL
                                  ]
                                ]
                                # logicalChannelList#
                                [
                                  allSizes# NULL
                                ]
                              }
                            ]
                          ]
                          # semistaticTF_Information#
                          {
                            channelCodingType#
                            [
                              convolutional# third
                            ]
                            # rateMatchingAttribute# 170 # crc_Size# crc16
                          }
                        }
                      ]
                    }
                  ]
                  # modeSpecificTransChInfo#
                  [
                    fdd#
                    {
                      cpch_SetID# OMIT# addReconfTransChDRAC_Info# OMIT
                    }
                  ]
                  # dl_CommonTransChInfo#
                  {
                    sccpch_TFCS# OMIT# modeSpecificInfo#
                    [
                      fdd#
                      {
                        dl_Parameters#
                        [
                          dl_DCH_TFCS#
                          [
                            normalTFCI_Signalling#
                            [
                              complete#
                              {
                                ctfcSize#
                                [
                                  ctfc4Bit#
                                  [
                                    {
                                      ctfc4# 0 # powerOffsetInformation# OMIT
                                    }
                                    #
                                    {
                                      ctfc4# 1 # powerOffsetInformation# OMIT
                                    }
                                    #
                                    {
                                      ctfc4# 2 # powerOffsetInformation# OMIT
                                    }
                                    #
                                    {
                                      ctfc4# 3 # powerOffsetInformation# OMIT
                                    }
                                    #
                                    {
                                      ctfc4# 4 # powerOffsetInformation# OMIT
                                    }
                                    #
                                    {
                                      ctfc4# 5 # powerOffsetInformation# OMIT
                                    }
                                    #
                                    {
                                      ctfc4# 6 # powerOffsetInformation# OMIT
                                    }
                                    #
                                    {
                                      ctfc4# 7 # powerOffsetInformation# OMIT
                                    }
                                    #
                                    {
                                      ctfc4# 8 # powerOffsetInformation# OMIT
                                    }
                                    #
                                    {
                                      ctfc4# 9 # powerOffsetInformation# OMIT
                                    }
                                  ]
                                ]
                              }
                            ]
                          ]
                        ]
                      }
                    ]
                  }
                  # dl_DeletedTransChInfoList# OMIT# dl_AddReconfTransChInfoList#
                  [
                    {
                      dl_TransportChannelType# dch# dl_transportChannelIdentity# 6 # tfs_SignallingMode#
                      [
                        sameAsULTrCH#
                        {
                          ul_TransportChannelType# dch# ul_TransportChannelIdentity# 1
                        }
                      ]
                      # dch_QualityTarget#
                      {
                        bler_QualityValue# #20
                      }
                      # dummy# OMIT
                    }
                    #
                    {
                      dl_TransportChannelType# dch# dl_transportChannelIdentity# 10 # tfs_SignallingMode#
                      [
                        sameAsULTrCH#
                        {
                          ul_TransportChannelType# dch# ul_TransportChannelIdentity# 5
                        }
                      ]
                      # dch_QualityTarget#
                      {
                        bler_QualityValue# #20
                      }
                      # dummy# OMIT
                    }
                  ]
                  # frequencyInfo# OMIT# maxAllowedUL_TX_Power# 33 # ul_ChannelRequirement#
                  [
                    ul_DPCH_Info#
                    {
                      ul_DPCH_PowerControlInfo#
                      [
                        fdd#
                        {
                          dpcch_PowerOffset# #40 # pc_Preamble# 1 # sRB_delay# 7 # powerControlAlgorithm#
                          [
                            algorithm1# 1
                          ]
                        }
                      ]
                      # modeSpecificInfo#
                      [
                        fdd#
                        {
                          scramblingCodeType# longSC# scramblingCode# 0 # numberOfDPDCH# OMIT# spreadingFactor# sf16# tfci_Existence# GcTRUE # numberOfFBI_Bits# OMIT# puncturingLimit# pl0_96
                        }
                      ]
                    }
                  ]
                  # modeSpecificPhysChInfo#
                  [
                    fdd#
                    {
                      dl_PDSCH_Information# OMIT
                    }
                  ]
                  # dl_CommonInformation#
                  {
                    dl_DPCH_InfoCommon#
                    {
                      cfnHandling#
                      [
                        maintain# NULL
                      ]
                      # modeSpecificInfo#
                      [
                        fdd#
                        {
                          dl_DPCH_PowerControlInfo#
                          {
                            modeSpecificInfo#
                            [
                              fdd#
                              {
                                dpc_Mode# singleTPC
                              }
                            ]
                          }
                          # powerOffsetPilot_pdpdch# 0 # dl_rate_matching_restriction# OMIT# spreadingFactorAndPilot#
                          [
                            sfd32# NULL
                          ]
                          # positionFixedOrFlexible# flexible# tfci_Existence# GcTRUE
                        }
                      ]
                    }
                    # modeSpecificInfo#
                    [
                      fdd#
                      {
                        defaultDPCH_OffsetValue# OMIT# dpch_CompressedModeInfo# OMIT# tx_DiversityMode# noDiversity# ssdt_Information# OMIT
                      }
                    ]
                  }
                  # dl_InformationPerRL_List#
                  [
                    {
                      modeSpecificInfo#
                      [
                        fdd#
                        {
                          primaryCPICH_Info#
                          {
                            primaryScramblingCode# 100
                          }
                          # pdsch_SHO_DCH_Info# OMIT# pdsch_CodeMapping# OMIT
                        }
                      ]
                      # dl_DPCH_InfoPerRL#
                      [
                        fdd#
                        {
                          pCPICH_UsageForChannelEst# mayBeUsed# dpch_FrameOffset# 0 # secondaryCPICH_Info# OMIT# dl_ChannelisationCodeList#
                          [
                            {
                              secondaryScramblingCode# 1 # sf_AndCodeNumber#
                              [
                                sf32# 0
                              ]
                              # scramblingCodeChange# OMIT
                            }
                          ]
                          # tpc_CombinationIndex# 0 # ssdt_CellIdentity# OMIT# closedLoopTimingAdjMode# OMIT
                        }
                      ]
                      # sccpch_InfoforFACH# OMIT
                    }
                  ]
                }
                # v3a0NonCriticalExtensions#
                {
                  radioBearerSetup_v3a0ext#
                  {
                    new_DSCH_RNTI# OMIT
                  }
                  # laterNonCriticalExtensions# OMIT
                }
              }
            ]
          ]
        }
      ]
    }

TTCN PDU: CPHY_RL_Modify_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 26
      ],
      ratType: fdd,
      modifyMessage:
      {
        activationTime:
        [
          activationCFN: 104
        ],
        physicalChannelInfo:
        [
          dPCHInfo:
          {
            ul_DPCHInfo: OMIT,
            dl_DPCHInfo:
            {
              dl_CommonInformation:
              {
                dl_DPCH_InfoCommon:
                {
                  cfnHandling:
                  [
                    maintain: NULL
                  ],
                  modeSpecificInfo:
                  [
                    fdd:
                    {
                      dl_DPCH_PowerControlInfo:
                      {
                        modeSpecificInfo:
                        [
                          fdd:
                          {
                            dpc_Mode: singleTPC
                          }
                        ]
                      },
                      powerOffsetPilot_pdpdch: 0,
                      dl_rate_matching_restriction: OMIT,
                      spreadingFactorAndPilot:
                      [
                        sfd32: NULL
                      ],
                      positionFixedOrFlexible: flexible,
                      tfci_Existence: GcTRUE
                    }
                  ]
                },
                modeSpecificInfo:
                [
                  fdd:
                  {
                    defaultDPCH_OffsetValue: OMIT,
                    dpch_CompressedModeInfo: OMIT,
                    tx_DiversityMode: noDiversity,
                    ssdt_Information: OMIT
                  }
                ]
              },
              dl_DPCH_InfoPerRL:
              [
                fdd:
                {
                  pCPICH_UsageForChannelEst: mayBeUsed,
                  dpch_FrameOffset: 0,
                  secondaryCPICH_Info: OMIT,
                  dl_ChannelisationCodeList:
                  [
                    {
                      secondaryScramblingCode: 1,
                      sf_AndCodeNumber:
                      [
                        sf32: 0
                      ],
                      scramblingCodeChange: OMIT
                    }
                  ],
                  tpc_CombinationIndex: 0,
                  ssdt_CellIdentity: OMIT,
                  closedLoopTimingAdjMode: OMIT
                }
              ],
              powerOffsetOfTFCI_PO1: 0,
              powerOffsetOfTPC_PO2: 0,
              powerOffsetOfPILOT_PO3: 0,
              dl_TxPower: -5,
              dl_TxPowerMax: 15,
              dl_TxPowerMin: -35
            }
          }
        ]
      }
    }

TTCN PDU: CPHY_TrCH_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 26
      ],
      ratType: fdd,
      trchConfigType:
      [
        dch: Normal
      ],
      configMessage:
      {
        activationTime:
        [
          activationCFN: 104
        ],
        ulconnectedTrCHList: OMIT,
        ulTFCS: OMIT,
        dlconnectedTrCHList:
        [
          {
            trchid: 6,
            dl_TransportChannelType: dch,
            transportChannelInfo:
            {
              tti:
              [
                tti20:
                [
                  {
                    tb_Size: 336,
                    numberOfTbSizeList:
                    [
                      [
                        zero: NULL
                      ],

                      [
                        one: NULL
                      ],

                      [
                        small: 2
                      ],

                      [
                        small: 3
                      ],

                      [
                        small: 4
                      ]
                    ],
                    logicalChannelList:
                    [
                      allSizes: NULL
                    ]
                  }
                ]
              ],
              semistaticTF_Information:
              {
                channelCodingType:
                [
                  turbo: NULL
                ],
                rateMatchingAttribute# 150 # crc_Size# crc16
              }
            }
          }
          #
          {
            trchid# 10 # dl_TransportChannelType# dch# transportChannelInfo#
            {
              tti#
              [
                tti40#
                [
                  {
                    tb_Size# 148 # numberOfTbSizeList#
                    [
                      [
                        zero# NULL
                      ]
                      #
                      [
                        one# NULL
                      ]
                    ]
                    # logicalChannelList#
                    [
                      allSizes# NULL
                    ]
                  }
                ]
              ]
              # semistaticTF_Information#
              {
                channelCodingType#
                [
                  convolutional# third
                ]
                # rateMatchingAttribute# 170 # crc_Size# crc16
              }
            }
          }
        ]
        # dlTFCS#
        [
          normalTFCI_Signalling#
          [
            complete#
            {
              ctfcSize#
              [
                ctfc4Bit#
                [
                  {
                    ctfc4# 0 # powerOffsetInformation#
                    {
                      gainFactorInformation#
                      [
                        computedGainFactors# 0
                      ]
                      # powerOffsetPp_m# OMIT
                    }
                  }
                  #
                  {
                    ctfc4# 1 # powerOffsetInformation#
                    {
                      gainFactorInformation#
                      [
                        computedGainFactors# 0
                      ]
                      # powerOffsetPp_m# OMIT
                    }
                  }
                  #
                  {
                    ctfc4# 2 # powerOffsetInformation#
                    {
                      gainFactorInformation#
                      [
                        computedGainFactors# 0
                      ]
                      # powerOffsetPp_m# OMIT
                    }
                  }
                  #
                  {
                    ctfc4# 3 # powerOffsetInformation#
                    {
                      gainFactorInformation#
                      [
                        computedGainFactors# 0
                      ]
                      # powerOffsetPp_m# OMIT
                    }
                  }
                  #
                  {
                    ctfc4# 4 # powerOffsetInformation#
                    {
                      gainFactorInformation#
                      [
                        computedGainFactors# 0
                      ]
                      # powerOffsetPp_m# OMIT
                    }
                  }
                  #
                  {
                    ctfc4# 5 # powerOffsetInformation#
                    {
                      gainFactorInformation#
                      [
                        computedGainFactors# 0
                      ]
                      # powerOffsetPp_m# OMIT
                    }
                  }
                  #
                  {
                    ctfc4# 6 # powerOffsetInformation#
                    {
                      gainFactorInformation#
                      [
                        computedGainFactors# 0
                      ]
                      # powerOffsetPp_m# OMIT
                    }
                  }
                  #
                  {
                    ctfc4# 7 # powerOffsetInformation#
                    {
                      gainFactorInformation#
                      [
                        computedGainFactors# 0
                      ]
                      # powerOffsetPp_m# OMIT
                    }
                  }
                  #
                  {
                    ctfc4# 8 # powerOffsetInformation#
                    {
                      gainFactorInformation#
                      [
                        computedGainFactors# 0
                      ]
                      # powerOffsetPp_m# OMIT
                    }
                  }
                  #
                  {
                    ctfc4# 9 # powerOffsetInformation#
                    {
                      gainFactorInformation#
                      [
                        signalledGainFactors#
                        {
                          modeSpecificInfo#
                          [
                            fdd#
                            {
                              gainFactorBetaC# 9
                            }
                          ]
                          # gainFactorBetaD# 15 # referenceTFC_ID# 0
                        }
                      ]
                      # powerOffsetPp_m# OMIT
                    }
                  }
                ]
              ]
            }
          ]
        ]
      }
    }

TTCN PDU: CPHY_TrCH_Config_CNF

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 26
      ]
    }

TTCN PDU: CMAC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        physicalChannelIdentity: 26
      ],
      ratType: fdd,
      configMessage:
      [
        reconfigure:
        {
          activationTime:
          [
            activationCFN: 104
          ],
          uE_Info:
          {
            u_RNTI: OMIT,
            c_RNTI: OMIT
          },
          trCHInfo:
          {
            ulconnectedTrCHList: OMIT,
            ulTFCS: OMIT,
            dlconnectedTrCHList:
            [
              {
                trchid: 6,
                transportChannelInfo:
                {
                  tti:
                  [
                    tti20:
                    [
                      {
                        tb_Size: 336,
                        numberOfTbSizeList:
                        [
                          [
                            zero: NULL
                          ],

                          [
                            one: NULL
                          ],

                          [
                            small: 2
                          ],

                          [
                            small: 3
                          ],

                          [
                            small: 4
                          ]
                        ],
                        logicalChannelList:
                        [
                          allSizes: NULL
                        ]
                      }
                    ]
                  ],
                  semistaticTF_Information:
                  {
                    channelCodingType:
                    [
                      turbo: NULL
                    ],
                    rateMatchingAttribute# 150 # crc_Size# crc16
                  }
                }
              }
              #
              {
                trchid# 10 # transportChannelInfo#
                {
                  tti#
                  [
                    tti40#
                    [
                      {
                        tb_Size# 148 # numberOfTbSizeList#
                        [
                          [
                            zero# NULL
                          ]
                          #
                          [
                            one# NULL
                          ]
                        ]
                        # logicalChannelList#
                        [
                          allSizes# NULL
                        ]
                      }
                    ]
                  ]
                  # semistaticTF_Information#
                  {
                    channelCodingType#
                    [
                      convolutional# third
                    ]
                    # rateMatchingAttribute# 170 # crc_Size# crc16
                  }
                }
              }
            ]
            # dlTFCS#
            [
              normalTFCI_Signalling#
              [
                complete#
                {
                  ctfcSize#
                  [
                    ctfc4Bit#
                    [
                      {
                        ctfc4# 0 # powerOffsetInformation#
                        {
                          gainFactorInformation#
                          [
                            computedGainFactors# 0
                          ]
                          # powerOffsetPp_m# OMIT
                        }
                      }
                      #
                      {
                        ctfc4# 1 # powerOffsetInformation#
                        {
                          gainFactorInformation#
                          [
                            computedGainFactors# 0
                          ]
                          # powerOffsetPp_m# OMIT
                        }
                      }
                      #
                      {
                        ctfc4# 2 # powerOffsetInformation#
                        {
                          gainFactorInformation#
                          [
                            computedGainFactors# 0
                          ]
                          # powerOffsetPp_m# OMIT
                        }
                      }
                      #
                      {
                        ctfc4# 3 # powerOffsetInformation#
                        {
                          gainFactorInformation#
                          [
                            computedGainFactors# 0
                          ]
                          # powerOffsetPp_m# OMIT
                        }
                      }
                      #
                      {
                        ctfc4# 4 # powerOffsetInformation#
                        {
                          gainFactorInformation#
                          [
                            computedGainFactors# 0
                          ]
                          # powerOffsetPp_m# OMIT
                        }
                      }
                      #
                      {
                        ctfc4# 5 # powerOffsetInformation#
                        {
                          gainFactorInformation#
                          [
                            computedGainFactors# 0
                          ]
                          # powerOffsetPp_m# OMIT
                        }
                      }
                      #
                      {
                        ctfc4# 6 # powerOffsetInformation#
                        {
                          gainFactorInformation#
                          [
                            computedGainFactors# 0
                          ]
                          # powerOffsetPp_m# OMIT
                        }
                      }
                      #
                      {
                        ctfc4# 7 # powerOffsetInformation#
                        {
                          gainFactorInformation#
                          [
                            computedGainFactors# 0
                          ]
                          # powerOffsetPp_m# OMIT
                        }
                      }
                      #
                      {
                        ctfc4# 8 # powerOffsetInformation#
                        {
                          gainFactorInformation#
                          [
                            computedGainFactors# 0
                          ]
                          # powerOffsetPp_m# OMIT
                        }
                      }
                      #
                      {
                        ctfc4# 9 # powerOffsetInformation#
                        {
                          gainFactorInformation#
                          [
                            signalledGainFactors#
                            {
                              modeSpecificInfo#
                              [
                                fdd#
                                {
                                  gainFactorBetaC# 9
                                }
                              ]
                              # gainFactorBetaD# 15 # referenceTFC_ID# 0
                            }
                          ]
                          # powerOffsetPp_m# OMIT
                        }
                      }
                    ]
                  ]
                }
              ]
            ]
          }
          # trCH_LogCHMapping#
          {
            ulconnectedTrCHList# OMIT# dlconnectedTrCHList#
            [
              {
                trchid# 6 # trCH_LogCHMappingList#
                [
                  {
                    logicalChannel_Mapping#
                    [
                      dl_LogicalChannelMapping#
                      {
                        macHeaderManipulation# normalMacHeader# dl_TransportChannelType# dch# logicalChannelIdentity# 7 # logicalChannelType# dTCH# rlc_SizeList#
                        [
                          configured# NULL
                        ]
                        # mac_LogicalChannelPriority# 8
                      }
                    ]
                    # rB_Identity# 20 # cn_DomainIdentity# OMIT
                  }
                ]
              }
              #
              {
                trchid# 10 # trCH_LogCHMappingList#
                [
                  {
                    logicalChannel_Mapping#
                    [
                      dl_LogicalChannelMapping#
                      {
                        macHeaderManipulation# normalMacHeader# dl_TransportChannelType# dch# logicalChannelIdentity# 1 # logicalChannelType# dCCH# rlc_SizeList#
                        [
                          configured# NULL
                        ]
                        # mac_LogicalChannelPriority# 1
                      }
                    ]
                    # rB_Identity# 1 # cn_DomainIdentity# OMIT
                  }
                  #
                  {
                    logicalChannel_Mapping#
                    [
                      dl_LogicalChannelMapping#
                      {
                        macHeaderManipulation# normalMacHeader# dl_TransportChannelType# dch# logicalChannelIdentity# 2 # logicalChannelType# dCCH# rlc_SizeList#
                        [
                          configured# NULL
                        ]
                        # mac_LogicalChannelPriority# 2
                      }
                    ]
                    # rB_Identity# 2 # cn_DomainIdentity# OMIT
                  }
                  #
                  {
                    logicalChannel_Mapping#
                    [
                      dl_LogicalChannelMapping#
                      {
                        macHeaderManipulation# normalMacHeader# dl_TransportChannelType# dch# logicalChannelIdentity# 3 # logicalChannelType# dCCH# rlc_SizeList#
                        [
                          configured# NULL
                        ]
                        # mac_LogicalChannelPriority# 3
                      }
                    ]
                    # rB_Identity# 3 # cn_DomainIdentity# OMIT
                  }
                  #
                  {
                    logicalChannel_Mapping#
                    [
                      dl_LogicalChannelMapping#
                      {
                        macHeaderManipulation# normalMacHeader# dl_TransportChannelType# dch# logicalChannelIdentity# 4 # logicalChannelType# dCCH# rlc_SizeList#
                        [
                          configured# NULL
                        ]
                        # mac_LogicalChannelPriority# 4
                      }
                    ]
                    # rB_Identity# 4 # cn_DomainIdentity# OMIT
                  }
                ]
              }
            ]
          }
        }
      ]
    }

TTCN PDU: CPHY_RL_Modify_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 20
      ],
      ratType: fdd,
      modifyMessage:
      {
        activationTime:
        [
          activationCFN: 104
        ],
        physicalChannelInfo:
        [
          dPCHInfo:
          {
            ul_DPCHInfo:
            {
              ul_DPCH_PowerControlInfo:
              [
                fdd:
                {
                  dpcch_PowerOffset: -40,
                  pc_Preamble: 1,
                  sRB_delay: 7,
                  powerControlAlgorithm:
                  [
                    algorithm1: 1
                  ]
                }
              ],
              modeSpecificInfo:
              [
                fdd:
                {
                  scramblingCodeType: longSC,
                  scramblingCode: 0,
                  numberOfDPDCH: OMIT,
                  spreadingFactor: sf16,
                  tfci_Existence: GcTRUE,
                  numberOfFBI_Bits: OMIT,
                  puncturingLimit: pl0_96
                }
              ]
            },
            dl_DPCHInfo: OMIT
          }
        ]
      }
    }

TTCN PDU: CPHY_TrCH_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 20
      ],
      ratType: fdd,
      trchConfigType:
      [
        dch: Normal
      ],
      configMessage:
      {
        activationTime:
        [
          activationCFN: 104
        ],
        ulconnectedTrCHList:
        [
          {
            trchid: 1,
            ul_TransportChannelType: dch,
            transportChannelInfo:
            {
              tti:
              [
                tti20:
                [
                  {
                    tb_Size: 336,
                    numberOfTbSizeList:
                    [
                      [
                        zero: NULL
                      ],

                      [
                        one: NULL
                      ],

                      [
                        small: 2
                      ],

                      [
                        small: 3
                      ],

                      [
                        small: 4
                      ]
                    ],
                    logicalChannelList:
                    [
                      allSizes: NULL
                    ]
                  }
                ]
              ],
              semistaticTF_Information:
              {
                channelCodingType:
                [
                  turbo: NULL
                ],
                rateMatchingAttribute# 150 # crc_Size# crc16
              }
            }
          }
          #
          {
            trchid# 5 # ul_TransportChannelType# dch# transportChannelInfo#
            {
              tti#
              [
                tti40#
                [
                  {
                    tb_Size# 148 # numberOfTbSizeList#
                    [
                      [
                        zero# NULL
                      ]
                      #
                      [
                        one# NULL
                      ]
                    ]
                    # logicalChannelList#
                    [
                      allSizes# NULL
                    ]
                  }
                ]
              ]
              # semistaticTF_Information#
              {
                channelCodingType#
                [
                  convolutional# third
                ]
                # rateMatchingAttribute# 170 # crc_Size# crc16
              }
            }
          }
        ]
        # ulTFCS#
        [
          normalTFCI_Signalling#
          [
            complete#
            {
              ctfcSize#
              [
                ctfc4Bit#
                [
                  {
                    ctfc4# 0 # powerOffsetInformation# OMIT
                  }
                  #
                  {
                    ctfc4# 1 # powerOffsetInformation# OMIT
                  }
                  #
                  {
                    ctfc4# 2 # powerOffsetInformation# OMIT
                  }
                  #
                  {
                    ctfc4# 3 # powerOffsetInformation# OMIT
                  }
                  #
                  {
                    ctfc4# 4 # powerOffsetInformation# OMIT
                  }
                  #
                  {
                    ctfc4# 5 # powerOffsetInformation# OMIT
                  }
                  #
                  {
                    ctfc4# 6 # powerOffsetInformation# OMIT
                  }
                  #
                  {
                    ctfc4# 7 # powerOffsetInformation# OMIT
                  }
                  #
                  {
                    ctfc4# 8 # powerOffsetInformation# OMIT
                  }
                  #
                  {
                    ctfc4# 9 # powerOffsetInformation# OMIT
                  }
                ]
              ]
            }
          ]
        ]
        # dlconnectedTrCHList# OMIT# dlTFCS# OMIT
      }
    }

TTCN PDU: CPHY_TrCH_Config_CNF

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 20
      ]
    }

TTCN PDU: CMAC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        physicalChannelIdentity: 20
      ],
      ratType: fdd,
      configMessage:
      [
        reconfigure:
        {
          activationTime:
          [
            activationCFN: 104
          ],
          uE_Info:
          {
            u_RNTI: OMIT,
            c_RNTI: OMIT
          },
          trCHInfo:
          {
            ulconnectedTrCHList:
            [
              {
                trchid: 1,
                transportChannelInfo:
                {
                  tti:
                  [
                    tti20:
                    [
                      {
                        tb_Size: 336,
                        numberOfTbSizeList:
                        [
                          [
                            zero: NULL
                          ],

                          [
                            one: NULL
                          ],

                          [
                            small: 2
                          ],

                          [
                            small: 3
                          ],

                          [
                            small: 4
                          ]
                        ],
                        logicalChannelList:
                        [
                          allSizes: NULL
                        ]
                      }
                    ]
                  ],
                  semistaticTF_Information:
                  {
                    channelCodingType:
                    [
                      turbo: NULL
                    ],
                    rateMatchingAttribute# 150 # crc_Size# crc16
                  }
                }
              }
              #
              {
                trchid# 5 # transportChannelInfo#
                {
                  tti#
                  [
                    tti40#
                    [
                      {
                        tb_Size# 148 # numberOfTbSizeList#
                        [
                          [
                            zero# NULL
                          ]
                          #
                          [
                            one# NULL
                          ]
                        ]
                        # logicalChannelList#
                        [
                          allSizes# NULL
                        ]
                      }
                    ]
                  ]
                  # semistaticTF_Information#
                  {
                    channelCodingType#
                    [
                      convolutional# third
                    ]
                    # rateMatchingAttribute# 170 # crc_Size# crc16
                  }
                }
              }
            ]
            # ulTFCS#
            [
              normalTFCI_Signalling#
              [
                complete#
                {
                  ctfcSize#
                  [
                    ctfc4Bit#
                    [
                      {
                        ctfc4# 0 # powerOffsetInformation# OMIT
                      }
                      #
                      {
                        ctfc4# 1 # powerOffsetInformation# OMIT
                      }
                      #
                      {
                        ctfc4# 2 # powerOffsetInformation# OMIT
                      }
                      #
                      {
                        ctfc4# 3 # powerOffsetInformation# OMIT
                      }
                      #
                      {
                        ctfc4# 4 # powerOffsetInformation# OMIT
                      }
                      #
                      {
                        ctfc4# 5 # powerOffsetInformation# OMIT
                      }
                      #
                      {
                        ctfc4# 6 # powerOffsetInformation# OMIT
                      }
                      #
                      {
                        ctfc4# 7 # powerOffsetInformation# OMIT
                      }
                      #
                      {
                        ctfc4# 8 # powerOffsetInformation# OMIT
                      }
                      #
                      {
                        ctfc4# 9 # powerOffsetInformation# OMIT
                      }
                    ]
                  ]
                }
              ]
            ]
            # dlconnectedTrCHList# OMIT# dlTFCS# OMIT
          }
          # trCH_LogCHMapping#
          {
            ulconnectedTrCHList#
            [
              {
                trchid# 1 # trCH_LogCHMappingList#
                [
                  {
                    logicalChannel_Mapping#
                    [
                      ul_LogicalChannelMapping#
                      {
                        macHeaderManipulation# normalMacHeader# ul_TransportChannelType# dch# logicalChannelIdentity# 7 # logicalChannelType# dTCH
                      }
                    ]
                    # rB_Identity# 20 # cn_DomainIdentity# OMIT
                  }
                ]
              }
              #
              {
                trchid# 5 # trCH_LogCHMappingList#
                [
                  {
                    logicalChannel_Mapping#
                    [
                      ul_LogicalChannelMapping#
                      {
                        macHeaderManipulation# normalMacHeader# ul_TransportChannelType# dch# logicalChannelIdentity# 1 # logicalChannelType# dCCH
                      }
                    ]
                    # rB_Identity# 1 # cn_DomainIdentity# OMIT
                  }
                  #
                  {
                    logicalChannel_Mapping#
                    [
                      ul_LogicalChannelMapping#
                      {
                        macHeaderManipulation# normalMacHeader# ul_TransportChannelType# dch# logicalChannelIdentity# 2 # logicalChannelType# dCCH
                      }
                    ]
                    # rB_Identity# 2 # cn_DomainIdentity# OMIT
                  }
                  #
                  {
                    logicalChannel_Mapping#
                    [
                      ul_LogicalChannelMapping#
                      {
                        macHeaderManipulation# normalMacHeader# ul_TransportChannelType# dch# logicalChannelIdentity# 3 # logicalChannelType# dCCH
                      }
                    ]
                    # rB_Identity# 3 # cn_DomainIdentity# OMIT
                  }
                  #
                  {
                    logicalChannel_Mapping#
                    [
                      ul_LogicalChannelMapping#
                      {
                        macHeaderManipulation# normalMacHeader# ul_TransportChannelType# dch# logicalChannelIdentity# 4 # logicalChannelType# dCCH
                      }
                    ]
                    # rB_Identity# 4 # cn_DomainIdentity# OMIT
                  }
                ]
              }
            ]
            # dlconnectedTrCHList# OMIT
          }
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 20
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          sS_rlc_Info:
          {
            sS_ul_RLC_Mode:
            [
              dl_AM_RLC_Mode:
              {
                inSequenceDelivery: GcTRUE,
                receivingWindowSize: rw128,
                dl_RLC_StatusInfo:
                {
                  timerStatusProhibit: tsp200,
                  timerEPC: OMIT,
                  missingPDU_Indicator: GcTRUE,
                  timerStatusPeriodic: OMIT
                }
              }
            ],
            sS_dl_RLC_Mode:
            {
              dl_PayloadSize: 320,
              dl_RLCModeInfo:
              [
                ul_AM_RLC_Mode:
                {
                  transmissionRLC_Discard:
                  [
                    noDiscard: dat15
                  ],
                  transmissionWindowSize: tw128,
                  timerRST: tr500,
                  max_RST: rst4,
                  pollingInfo:
                  {
                    timerPollProhibit: tpp200,
                    timerPoll: tp200,
                    poll_PDU: OMIT,
                    poll_SDU: sdu1,
                    lastTransmissionPDU_Poll: GcTRUE,
                    lastRetransmissionPDU_Poll: GcTRUE,
                    pollWindow: pw99,
                    timerPollPeriodic: OMIT
                  }
                }
              ]
            }
          },
          rB_LogCH_Mapping:
          {
            uLlogicalChannelIdentity: 7,
            dLlogicalChannelIdentity: 7,
            logicalChannelType: OMIT,
            cn_DomainIdentity: OMIT
          }
        }
      ]
    }

TTCN PDU: RLC_AM_DATA_IND

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 2
      ],
      integrityResult:
      [
        integrityUsed: i_pass
      ],
      aM_message:
      [
        uL_DCCH_Message: PDU:
        {
          integrityCheckInfo:
          {
            messageAuthenticationCode: '10101010101011110011101101011001'B,
            rrc_MessageSequenceNumber: 2
          },
          message:
          [
            radioBearerSetupComplete:
            {
              rrc_TransactionIdentifier: 0,
              ul_IntegProtActivationInfo: OMIT,
              ul_TimingAdvance: OMIT,
              start_Value: '00000000000000000010'B,
              count_C_ActivationTime: OMIT,
              rb_UL_CiphActivationTimeInfo: OMIT,
              ul_CounterSynchronisationInfo: OMIT,
              laterNonCriticalExtensions: OMIT
            }
          ]
        }
      ]
    }

TTCN PDU: CRLC_SecurityMode_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      rlcSecurityInfo:
      {
        cn_DomainIdentity: ps_domain,
        startValue: '00000000000000000010'B,
        cipheringKey: OMIT,
        integrityKey: OMIT,
        gsmCipheringKey: OMIT
      }
    }

TTCN PDU: RRC_DataReq

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      rB_Id: 3,
      ch: OMIT,
      sapId: OMIT,
      cN_Domain: 1,
      msg: PDU:
      {
        ti:
        {
          tiFlag: '1'B,
          tiVal: '000'B
        },
        sM_ProtocolDiscriminator: '1010'B,
        msgType: '01000010'B,
        negiotiatedLLC_SAPI:
        {
          spare: '0000'B,
          nSAPI_Value: '0000'B
        },
        negiotiatedQoS:
        {
          length: '0B'O,
          spare: '00'B,
          dlyClass: '011'B,
          relabilityClass: '011'B,
          peakThroughput: '0100'B,
          spare1: '0'B,
          precedenceClass: '011'B,
          spare2: '000'B,
          meanThroughput: '11111'B,
          trafficClass: '011'B,
          deliveryOrder: '01'B,
          deliveryErrorSDU: '010'B,
          maxSDUSize: '20'O,
          maxBitRateUplink: '40'O,
          maxBitRateDnlink: '40'O,
          residualBER: '0111'B,
          sduErrRatio: '0100'B,
          transDly: '111111'B,
          trafficHandpro: '11'B,
          bitRateUplink: '10'O,
          bitRateDnlink: '10'O
        },
        spare: '0000'B,
        radioPriority:
        {
          spare: '0'B,
          value: '001'B
        },
        pDP_Address: OMIT,
        protocolConfOpts: OMIT,
        pktFlowID:
        {
          iei: '00110100'B,
          length: '01'O,
          pktFlowIdentifier: '00'O
        }
      }
    }

TTCN PDU: AT_CmdCnf

(To search, click here and then press Ctrl+F)

    {
      result: OMIT,
      resultString: "<CR><LF>OK<CR><LF>",
      sMS_BlockMode: OMIT
    }

TTCN PDU: RLC_AM_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 2
      ],
      confirmationRequest:
      [
        noConfirmationRequest: NULL
      ],
      aM_message:
      [
        dL_DCCH_Message: PDU:
        {
          integrityCheckInfo:
          {
            messageAuthenticationCode: '10110100100100010011100110111110'B,
            rrc_MessageSequenceNumber: 3
          },
          message:
          [
            measurementControl:
            [
              r3:
              {
                measurementControl_r3:
                {
                  rrc_TransactionIdentifier: 0,
                  measurementIdentity: 4,
                  measurementCommand:
                  [
                    setup:
                    [
                      interFrequencyMeasurement:
                      {
                        interFreqCellInfoList:
                        {
                          removedInterFreqCellList: OMIT,
                          newInterFreqCellList:
                          [
                            {
                              interFreqCellID: 3,
                              frequencyInfo:
                              {
                                modeSpecificInfo:
                                [
                                  fdd:
                                  {
                                    uarfcn_UL: OMIT,
                                    uarfcn_DL: 10837
                                  }
                                ]
                              },
                              cellInfo:
                              {
                                cellIndividualOffset: OMIT,
                                referenceTimeDifferenceToCell: OMIT,
                                modeSpecificInfo:
                                [
                                  fdd:
                                  {
                                    primaryCPICH_Info:
                                    {
                                      primaryScramblingCode: 250
                                    },
                                    primaryCPICH_TX_Power: OMIT,
                                    readSFN_Indicator: GcFALSE,
                                    tx_DiversityIndicator: GcFALSE
                                  }
                                ]
                              }
                            }
                          ],
                          cellsForInterFreqMeasList: OMIT
                        },
                        interFreqMeasQuantity:
                        {
                          reportingCriteria:
                          [
                            interFreqReportingCriteria:
                            {
                              filterCoefficient: fc4,
                              modeSpecificInfo:
                              [
                                fdd:
                                {
                                  freqQualityEstimateQuantity_FDD: cpich_RSCP
                                }
                              ]
                            }
                          ]
                        },
                        interFreqReportingQuantity:
                        {
                          utra_Carrier_RSSI: GcFALSE,
                          frequencyQualityEstimate: GcFALSE,
                          nonFreqRelatedQuantities:
                          {
                            dummy: noReport,
                            cellIdentity_reportingIndicator: GcFALSE,
                            cellSynchronisationInfoReportingIndicator: GcFALSE,
                            modeSpecificInfo:
                            [
                              fdd:
                              {
                                cpich_Ec_N0_reportingIndicator: GcFALSE,
                                cpich_RSCP_reportingIndicator: GcTRUE,
                                pathloss_reportingIndicator: GcFALSE
                              }
                            ]
                          }
                        },
                        measurementValidity: OMIT,
                        interFreqSetUpdate:
                        [
                          onWithNoReporting: NULL
                        ],
                        reportCriteria:
                        [
                          interFreqReportingCriteria:
                          {
                            interFreqEventList:
                            [
                              [
                                event2e:
                                {
                                  hysteresis: 1,
                                  timeToTrigger: ttt5000,
                                  reportingCellStatus: OMIT,
                                  nonUsedFreqParameterList:
                                  [
                                    {
                                      nonUsedFreqThreshold: -70,
                                      nonUsedFreqW: 0
                                    }
                                  ]
                                }
                              ],

                              [
                                event2b:
                                {
                                  usedFreqThreshold: -70,
                                  usedFreqW: 4,
                                  hysteresis: 1,
                                  timeToTrigger: ttt5000,
                                  reportingCellStatus:
                                  [
                                    withinActSetOrVirtualActSet_InterRATcells: e1
                                  ],
                                  nonUsedFreqParameterList:
                                  [
                                    {
                                      nonUsedFreqThreshold: -70,
                                      nonUsedFreqW: 0
                                    }
                                  ]
                                }
                              ]
                            ]
                          }
                        ]
                      }
                    ]
                  ],
                  measurementReportingMode:
                  {
                    measurementReportTransferMode: unacknowledgedModeRLC,
                    periodicalOrEventTrigger: eventTrigger
                  },
                  additionalMeasurementList: OMIT,
                  dpch_CompressedModeStatusInfo: OMIT
                },
                v390nonCriticalExtensions: OMIT
              }
            ]
          ]
        }
      ]
    }

TTCN PDU: CPHY_Frame_Number_CNF

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 26
      ],
      frameNumber: 144
    }

TTCN PDU: RLC_AM_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 2
      ],
      confirmationRequest:
      [
        noConfirmationRequest: NULL
      ],
      aM_message:
      [
        dL_DCCH_Message: PDU:
        {
          integrityCheckInfo:
          {
            messageAuthenticationCode: '10111010100011100010001011001110'B,
            rrc_MessageSequenceNumber: 4
          },
          message:
          [
            physicalChannelReconfiguration:
            [
              r3:
              {
                physicalChannelReconfiguration_r3:
                {
                  rrc_TransactionIdentifier: 0,
                  integrityProtectionModeInfo: OMIT,
                  cipheringModeInfo: OMIT,
                  activationTime: 136,
                  new_U_RNTI: OMIT,
                  new_C_RNTI: OMIT,
                  rrc_StateIndicator: cell_DCH,
                  utran_DRX_CycleLengthCoeff: OMIT,
                  cn_InformationInfo: OMIT,
                  ura_Identity: OMIT,
                  dl_CounterSynchronisationInfo: OMIT,
                  frequencyInfo:
                  {
                    modeSpecificInfo:
                    [
                      fdd:
                      {
                        uarfcn_UL: OMIT,
                        uarfcn_DL: 10700
                      }
                    ]
                  },
                  maxAllowedUL_TX_Power: 33,
                  ul_ChannelRequirement:
                  [
                    ul_DPCH_Info:
                    {
                      ul_DPCH_PowerControlInfo:
                      [
                        fdd:
                        {
                          dpcch_PowerOffset: -40,
                          pc_Preamble: 1,
                          sRB_delay: 7,
                          powerControlAlgorithm:
                          [
                            algorithm1: 1
                          ]
                        }
                      ],
                      modeSpecificInfo:
                      [
                        fdd:
                        {
                          scramblingCodeType: longSC,
                          scramblingCode: 0,
                          numberOfDPDCH: OMIT,
                          spreadingFactor: sf16,
                          tfci_Existence: GcTRUE,
                          numberOfFBI_Bits: OMIT,
                          puncturingLimit: pl0_96
                        }
                      ]
                    }
                  ],
                  modeSpecificInfo:
                  [
                    fdd:
                    {
                      dl_PDSCH_Information: OMIT
                    }
                  ],
                  dl_CommonInformation:
                  {
                    dl_DPCH_InfoCommon:
                    {
                      cfnHandling:
                      [
                        maintain: NULL
                      ],
                      modeSpecificInfo:
                      [
                        fdd:
                        {
                          dl_DPCH_PowerControlInfo:
                          {
                            modeSpecificInfo:
                            [
                              fdd:
                              {
                                dpc_Mode: singleTPC
                              }
                            ]
                          },
                          powerOffsetPilot_pdpdch: 0,
                          dl_rate_matching_restriction: OMIT,
                          spreadingFactorAndPilot:
                          [
                            sfd32: NULL
                          ],
                          positionFixedOrFlexible: flexible,
                          tfci_Existence: GcTRUE
                        }
                      ]
                    },
                    modeSpecificInfo:
                    [
                      fdd:
                      {
                        defaultDPCH_OffsetValue: 0,
                        dpch_CompressedModeInfo:
                        {
                          tgp_SequenceList:
                          [
                            {
                              tgpsi: 1,
                              tgps_Status:
                              [
                                activate:
                                {
                                  tgcfn: 140
                                }
                              ],
                              tgps_ConfigurationParams:
                              {
                                tgmp: fdd_Measurement,
                                tgprc: 0,
                                tgsn: 4,
                                tgl1: 7,
                                tgl2: OMIT,
                                tgd: 270,
                                tgpl1: 3,
                                tgpl2: OMIT,
                                rpp: mode0,
                                itp: mode0,
                                ul_DL_Mode:
                                [
                                  ul_and_dl:
                                  {
                                    ul: sf_2,
                                    dl: sf_2
                                  }
                                ],
                                dl_FrameType: dl_FrameTypeA,
                                deltaSIR1: 2,
                                deltaSIRAfter1: 1,
                                deltaSIR2: OMIT,
                                deltaSIRAfter2: OMIT,
                                nidentifyAbort: OMIT,
                                treconfirmAbort: OMIT
                              }
                            }
                          ]
                        },
                        tx_DiversityMode: noDiversity,
                        ssdt_Information: OMIT
                      }
                    ]
                  },
                  dl_InformationPerRL_List:
                  [
                    {
                      modeSpecificInfo:
                      [
                        fdd:
                        {
                          primaryCPICH_Info:
                          {
                            primaryScramblingCode: 100
                          },
                          pdsch_SHO_DCH_Info: OMIT,
                          pdsch_CodeMapping: OMIT
                        }
                      ],
                      dl_DPCH_InfoPerRL:
                      [
                        fdd:
                        {
                          pCPICH_UsageForChannelEst: mayBeUsed,
                          dpch_FrameOffset: 0,
                          secondaryCPICH_Info: OMIT,
                          dl_ChannelisationCodeList:
                          [
                            {
                              secondaryScramblingCode: 5,
                              sf_AndCodeNumber:
                              [
                                sf32: 0
                              ],
                              scramblingCodeChange: OMIT
                            }
                          ],
                          tpc_CombinationIndex: 0,
                          ssdt_CellIdentity: OMIT,
                          closedLoopTimingAdjMode: OMIT
                        }
                      ],
                      sccpch_InfoforFACH: OMIT
                    }
                  ]
                },
                v3a0NonCriticalExtensions: OMIT
              }
            ]
          ]
        }
      ]
    }

TTCN PDU: CPHY_RL_Modify_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 26
      ],
      ratType: fdd,
      modifyMessage:
      {
        activationTime:
        [
          activationCFN: 136
        ],
        physicalChannelInfo:
        [
          dPCHInfo:
          {
            ul_DPCHInfo: OMIT,
            dl_DPCHInfo:
            {
              dl_CommonInformation:
              {
                dl_DPCH_InfoCommon:
                {
                  cfnHandling:
                  [
                    maintain: NULL
                  ],
                  modeSpecificInfo:
                  [
                    fdd:
                    {
                      dl_DPCH_PowerControlInfo:
                      {
                        modeSpecificInfo:
                        [
                          fdd:
                          {
                            dpc_Mode: singleTPC
                          }
                        ]
                      },
                      powerOffsetPilot_pdpdch: 0,
                      dl_rate_matching_restriction: OMIT,
                      spreadingFactorAndPilot:
                      [
                        sfd32: NULL
                      ],
                      positionFixedOrFlexible: flexible,
                      tfci_Existence: GcTRUE
                    }
                  ]
                },
                modeSpecificInfo:
                [
                  fdd:
                  {
                    defaultDPCH_OffsetValue: 0,
                    dpch_CompressedModeInfo:
                    {
                      tgp_SequenceList:
                      [
                        {
                          tgpsi: 1,
                          tgps_Status:
                          [
                            activate:
                            {
                              tgcfn: 140
                            }
                          ],
                          tgps_ConfigurationParams:
                          {
                            tgmp: fdd_Measurement,
                            tgprc: 0,
                            tgsn: 4,
                            tgl1: 7,
                            tgl2: OMIT,
                            tgd: 270,
                            tgpl1: 3,
                            tgpl2: OMIT,
                            rpp: mode0,
                            itp: mode0,
                            ul_DL_Mode:
                            [
                              ul_and_dl:
                              {
                                ul: sf_2,
                                dl: sf_2
                              }
                            ],
                            dl_FrameType: dl_FrameTypeA,
                            deltaSIR1: 2,
                            deltaSIRAfter1: 1,
                            deltaSIR2: OMIT,
                            deltaSIRAfter2: OMIT,
                            nidentifyAbort: OMIT,
                            treconfirmAbort: OMIT
                          }
                        }
                      ]
                    },
                    tx_DiversityMode: noDiversity,
                    ssdt_Information: OMIT
                  }
                ]
              },
              dl_DPCH_InfoPerRL:
              [
                fdd:
                {
                  pCPICH_UsageForChannelEst: mayBeUsed,
                  dpch_FrameOffset: 0,
                  secondaryCPICH_Info: OMIT,
                  dl_ChannelisationCodeList:
                  [
                    {
                      secondaryScramblingCode: 5,
                      sf_AndCodeNumber:
                      [
                        sf32: 0
                      ],
                      scramblingCodeChange: noCodeChange
                    }
                  ],
                  tpc_CombinationIndex: 0,
                  ssdt_CellIdentity: OMIT,
                  closedLoopTimingAdjMode: OMIT
                }
              ],
              powerOffsetOfTFCI_PO1: 0,
              powerOffsetOfTPC_PO2: 0,
              powerOffsetOfPILOT_PO3: 0,
              dl_TxPower: -5,
              dl_TxPowerMax: 15,
              dl_TxPowerMin: -35
            }
          }
        ]
      }
    }

TTCN PDU: CPHY_RL_Modify_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 20
      ],
      ratType: fdd,
      modifyMessage:
      {
        activationTime:
        [
          activationCFN: 136
        ],
        physicalChannelInfo:
        [
          dPCHInfo:
          {
            ul_DPCHInfo:
            {
              ul_DPCH_PowerControlInfo:
              [
                fdd:
                {
                  dpcch_PowerOffset: -40,
                  pc_Preamble: 1,
                  sRB_delay: 7,
                  powerControlAlgorithm:
                  [
                    algorithm1: 1
                  ]
                }
              ],
              modeSpecificInfo:
              [
                fdd:
                {
                  scramblingCodeType: longSC,
                  scramblingCode: 0,
                  numberOfDPDCH: OMIT,
                  spreadingFactor: sf16,
                  tfci_Existence: GcTRUE,
                  numberOfFBI_Bits: OMIT,
                  puncturingLimit: pl0_96
                }
              ]
            },
            dl_DPCHInfo: OMIT
          }
        ]
      }
    }

TTCN PDU: RLC_AM_DATA_IND

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 2
      ],
      integrityResult:
      [
        integrityUsed: i_pass
      ],
      aM_message:
      [
        uL_DCCH_Message: PDU:
        {
          integrityCheckInfo:
          {
            messageAuthenticationCode: '00010011111100011101100011010111'B,
            rrc_MessageSequenceNumber: 3
          },
          message:
          [
            physicalChannelReconfigurationComplete:
            {
              rrc_TransactionIdentifier: 0,
              ul_IntegProtActivationInfo: OMIT,
              ul_TimingAdvance: OMIT,
              count_C_ActivationTime: OMIT,
              rb_UL_CiphActivationTimeInfo: OMIT,
              ul_CounterSynchronisationInfo: OMIT,
              laterNonCriticalExtensions: OMIT
            }
          ]
        }
      ]
    }

TTCN PDU: RLC_UM_DATA_IND

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 1
      ],
      integrityResult:
      [
        integrityUsed: i_pass
      ],
      uM_message:
      [
        uL_DCCH_Message: PDU:
        {
          integrityCheckInfo:
          {
            messageAuthenticationCode: '10001100010111011100000101000001'B,
            rrc_MessageSequenceNumber: 1
          },
          message:
          [
            measurementReport:
            {
              measurementIdentity: 4,
              measuredResults: OMIT,
              measuredResultsOnRACH: OMIT,
              additionalMeasuredResults: OMIT,
              eventResults:
              [
                interFreqEventResults:
                {
                  eventID: e2e,
                  interFreqCellList:
                  [
                    {
                      frequencyInfo:
                      {
                        modeSpecificInfo:
                        [
                          fdd:
                          {
                            uarfcn_UL: OMIT,
                            uarfcn_DL: 10837
                          }
                        ]
                      },
                      nonFreqRelatedEventResults:
                      [
                        fdd:
                        [
                          {
                            primaryScramblingCode: 250
                          }
                        ]
                      ]
                    }
                  ]
                }
              ],
              v390nonCriticalExtensions: OMIT
            }
          ]
        }
      ]
    }

TTCN PDU: RLC_UM_DATA_IND

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 1
      ],
      integrityResult:
      [
        integrityUsed: i_pass
      ],
      uM_message:
      [
        uL_DCCH_Message: PDU:
        {
          integrityCheckInfo:
          {
            messageAuthenticationCode: '01101111000101011100010000110101'B,
            rrc_MessageSequenceNumber: 2
          },
          message:
          [
            measurementReport:
            {
              measurementIdentity: 4,
              measuredResults:
              [
                interFreqMeasuredResultsList:
                [
                  {
                    frequencyInfo:
                    {
                      modeSpecificInfo:
                      [
                        fdd:
                        {
                          uarfcn_UL: OMIT,
                          uarfcn_DL: 10837
                        }
                      ]
                    },
                    utra_CarrierRSSI: OMIT,
                    interFreqCellMeasuredResultsList:
                    [
                      {
                        cellIdentity: OMIT,
                        dummy: OMIT,
                        cellSynchronisationInfo: OMIT,
                        modeSpecificInfo:
                        [
                          fdd:
                          {
                            primaryCPICH_Info:
                            {
                              primaryScramblingCode: 250
                            },
                            cpich_Ec_N0: OMIT,
                            cpich_RSCP: 55,
                            pathloss: OMIT
                          }
                        ]
                      }
                    ]
                  }
                ]
              ],
              measuredResultsOnRACH: OMIT,
              additionalMeasuredResults: OMIT,
              eventResults:
              [
                interFreqEventResults:
                {
                  eventID: e2b,
                  interFreqCellList:
                  [
                    {
                      frequencyInfo:
                      {
                        modeSpecificInfo:
                        [
                          fdd:
                          {
                            uarfcn_UL: OMIT,
                            uarfcn_DL: 10837
                          }
                        ]
                      },
                      nonFreqRelatedEventResults:
                      [
                        fdd:
                        [
                          {
                            primaryScramblingCode: 250
                          }
                        ]
                      ]
                    }
                  ]
                }
              ],
              v390nonCriticalExtensions: OMIT
            }
          ]
        }
      ]
    }

TTCN PDU: RLC_UM_DATA_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 1
      ],
      uM_message:
      [
        dL_DCCH_Message: PDU:
        {
          integrityCheckInfo:
          {
            messageAuthenticationCode: '11101100100111000001011111010011'B,
            rrc_MessageSequenceNumber: 1
          },
          message:
          [
            rrcConnectionRelease:
            [
              r3:
              {
                rrcConnectionRelease_r3:
                {
                  rrc_TransactionIdentifier: 0,
                  n_308: 1,
                  releaseCause: normalEvent,
                  rplmn_information: OMIT
                },
                laterNonCriticalExtensions: OMIT
              }
            ]
          ]
        }
      ],
      specialLI: GcFALSE
    }

TTCN PDU: RLC_UM_DATA_IND

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 1
      ],
      integrityResult:
      [
        integrityUsed: i_pass
      ],
      uM_message:
      [
        uL_DCCH_Message: PDU:
        {
          integrityCheckInfo:
          {
            messageAuthenticationCode: '01100011110001101001000110000100'B,
            rrc_MessageSequenceNumber: 3
          },
          message:
          [
            rrcConnectionReleaseComplete:
            {
              rrc_TransactionIdentifier: 0,
              errorIndication: OMIT,
              laterNonCriticalExtensions: OMIT
            }
          ]
        }
      ]
    }

TTCN PDU: RLC_UM_DATA_IND

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 1
      ],
      integrityResult:
      [
        integrityUsed: i_pass
      ],
      uM_message:
      [
        uL_DCCH_Message: PDU:
        {
          integrityCheckInfo:
          {
            messageAuthenticationCode: '00101011001011111001011000101110'B,
            rrc_MessageSequenceNumber: 4
          },
          message:
          [
            rrcConnectionReleaseComplete:
            {
              rrc_TransactionIdentifier: 0,
              errorIndication: OMIT,
              laterNonCriticalExtensions: OMIT
            }
          ]
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 1
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 2
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 3
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 4
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 20
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CMAC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        physicalChannelIdentity: 26
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CMAC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        physicalChannelIdentity: 20
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CPHY_TrCH_Release_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 26
      ],
      trchConfigType:
      [
        dch: Normal
      ]
    }

TTCN PDU: CPHY_TrCH_Release_CNF

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 26
      ]
    }

TTCN PDU: CPHY_TrCH_Release_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 20
      ],
      trchConfigType:
      [
        dch: Normal
      ]
    }

TTCN PDU: CPHY_TrCH_Release_CNF

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 20
      ]
    }

TTCN PDU: CPHY_RL_Setup_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 26
      ],
      ratType: fdd,
      setupMessage:
      {
        physicalChannelInfo:
        [
          dPCHInfo:
          {
            ul_DPCHInfo: OMIT,
            dl_DPCHInfo:
            {
              dl_CommonInformation:
              {
                dl_DPCH_InfoCommon:
                {
                  cfnHandling:
                  [
                    initialise:
                    {
                      cfntargetsfnframeoffset: OMIT
                    }
                  ],
                  modeSpecificInfo:
                  [
                    fdd:
                    {
                      dl_DPCH_PowerControlInfo:
                      {
                        modeSpecificInfo:
                        [
                          fdd:
                          {
                            dpc_Mode: singleTPC
                          }
                        ]
                      },
                      powerOffsetPilot_pdpdch: 0,
                      dl_rate_matching_restriction: OMIT,
                      spreadingFactorAndPilot:
                      [
                        sfd128: pb4
                      ],
                      positionFixedOrFlexible: fixed,
                      tfci_Existence: GcFALSE
                    }
                  ]
                },
                modeSpecificInfo:
                [
                  fdd:
                  {
                    defaultDPCH_OffsetValue: 0,
                    dpch_CompressedModeInfo: OMIT,
                    tx_DiversityMode: noDiversity,
                    ssdt_Information: OMIT
                  }
                ]
              },
              dl_DPCH_InfoPerRL:
              [
                fdd:
                {
                  pCPICH_UsageForChannelEst: mayBeUsed,
                  dpch_FrameOffset: 0,
                  secondaryCPICH_Info: OMIT,
                  dl_ChannelisationCodeList:
                  [
                    {
                      secondaryScramblingCode: 1,
                      sf_AndCodeNumber:
                      [
                        sf128: 0
                      ],
                      scramblingCodeChange: OMIT
                    }
                  ],
                  tpc_CombinationIndex: 0,
                  ssdt_CellIdentity: OMIT,
                  closedLoopTimingAdjMode: OMIT
                }
              ],
              powerOffsetOfTFCI_PO1: 0,
              powerOffsetOfTPC_PO2: 0,
              powerOffsetOfPILOT_PO3: 0,
              dl_TxPower: -5,
              dl_TxPowerMax: 15,
              dl_TxPowerMin: -35
            }
          }
        ]
      }
    }

TTCN PDU: CPHY_TrCH_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 26
      ],
      ratType: fdd,
      trchConfigType:
      [
        dch: Normal
      ],
      configMessage:
      {
        activationTime:
        [
          activateNow: NULL
        ],
        ulconnectedTrCHList: OMIT,
        ulTFCS: OMIT,
        dlconnectedTrCHList:
        [
          {
            trchid: 10,
            dl_TransportChannelType: dch,
            transportChannelInfo:
            {
              tti:
              [
                tti10:
                [
                  {
                    tb_Size: 148,
                    numberOfTbSizeList:
                    [
                      [
                        zero: NULL
                      ],

                      [
                        one: NULL
                      ]
                    ],
                    logicalChannelList:
                    [
                      allSizes: NULL
                    ]
                  }
                ]
              ],
              semistaticTF_Information:
              {
                channelCodingType:
                [
                  convolutional: third
                ],
                rateMatchingAttribute# 192 # crc_Size# crc16
              }
            }
          }
        ]
        # dlTFCS#
        [
          normalTFCI_Signalling#
          [
            complete#
            {
              ctfcSize#
              [
                ctfc2Bit#
                [
                  {
                    ctfc2# 0 # powerOffsetInformation#
                    {
                      gainFactorInformation#
                      [
                        computedGainFactors# 0
                      ]
                      # powerOffsetPp_m# OMIT
                    }
                  }
                  #
                  {
                    ctfc2# 1 # powerOffsetInformation#
                    {
                      gainFactorInformation#
                      [
                        signalledGainFactors#
                        {
                          modeSpecificInfo#
                          [
                            fdd#
                            {
                              gainFactorBetaC# 11
                            }
                          ]
                          # gainFactorBetaD# 15 # referenceTFC_ID# 0
                        }
                      ]
                      # powerOffsetPp_m# OMIT
                    }
                  }
                ]
              ]
            }
          ]
        ]
      }
    }

TTCN PDU: CPHY_TrCH_Config_CNF

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 26
      ]
    }

TTCN PDU: CMAC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        physicalChannelIdentity: 26
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          activationTime:
          [
            activateNow: NULL
          ],
          uE_Info:
          {
            u_RNTI: OMIT,
            c_RNTI: OMIT
          },
          trCHInfo:
          {
            ulconnectedTrCHList: OMIT,
            ulTFCS: OMIT,
            dlconnectedTrCHList:
            [
              {
                trchid: 10,
                transportChannelInfo:
                {
                  tti:
                  [
                    tti10:
                    [
                      {
                        tb_Size: 148,
                        numberOfTbSizeList:
                        [
                          [
                            zero: NULL
                          ],

                          [
                            one: NULL
                          ]
                        ],
                        logicalChannelList:
                        [
                          allSizes: NULL
                        ]
                      }
                    ]
                  ],
                  semistaticTF_Information:
                  {
                    channelCodingType:
                    [
                      convolutional: third
                    ],
                    rateMatchingAttribute# 192 # crc_Size# crc16
                  }
                }
              }
            ]
            # dlTFCS#
            [
              normalTFCI_Signalling#
              [
                complete#
                {
                  ctfcSize#
                  [
                    ctfc2Bit#
                    [
                      {
                        ctfc2# 0 # powerOffsetInformation#
                        {
                          gainFactorInformation#
                          [
                            computedGainFactors# 0
                          ]
                          # powerOffsetPp_m# OMIT
                        }
                      }
                      #
                      {
                        ctfc2# 1 # powerOffsetInformation#
                        {
                          gainFactorInformation#
                          [
                            signalledGainFactors#
                            {
                              modeSpecificInfo#
                              [
                                fdd#
                                {
                                  gainFactorBetaC# 11
                                }
                              ]
                              # gainFactorBetaD# 15 # referenceTFC_ID# 0
                            }
                          ]
                          # powerOffsetPp_m# OMIT
                        }
                      }
                    ]
                  ]
                }
              ]
            ]
          }
          # trCH_LogCHMapping#
          {
            ulconnectedTrCHList# OMIT# dlconnectedTrCHList#
            [
              {
                trchid# 10 # trCH_LogCHMappingList#
                [
                  {
                    logicalChannel_Mapping#
                    [
                      dl_LogicalChannelMapping#
                      {
                        macHeaderManipulation# normalMacHeader# dl_TransportChannelType# dch# logicalChannelIdentity# 1 # logicalChannelType# dCCH# rlc_SizeList#
                        [
                          configured# NULL
                        ]
                        # mac_LogicalChannelPriority# 1
                      }
                    ]
                    # rB_Identity# 1 # cn_DomainIdentity# OMIT
                  }
                  #
                  {
                    logicalChannel_Mapping#
                    [
                      dl_LogicalChannelMapping#
                      {
                        macHeaderManipulation# normalMacHeader# dl_TransportChannelType# dch# logicalChannelIdentity# 2 # logicalChannelType# dCCH# rlc_SizeList#
                        [
                          configured# NULL
                        ]
                        # mac_LogicalChannelPriority# 2
                      }
                    ]
                    # rB_Identity# 2 # cn_DomainIdentity# OMIT
                  }
                  #
                  {
                    logicalChannel_Mapping#
                    [
                      dl_LogicalChannelMapping#
                      {
                        macHeaderManipulation# normalMacHeader# dl_TransportChannelType# dch# logicalChannelIdentity# 3 # logicalChannelType# dCCH# rlc_SizeList#
                        [
                          configured# NULL
                        ]
                        # mac_LogicalChannelPriority# 3
                      }
                    ]
                    # rB_Identity# 3 # cn_DomainIdentity# OMIT
                  }
                  #
                  {
                    logicalChannel_Mapping#
                    [
                      dl_LogicalChannelMapping#
                      {
                        macHeaderManipulation# normalMacHeader# dl_TransportChannelType# dch# logicalChannelIdentity# 4 # logicalChannelType# dCCH# rlc_SizeList#
                        [
                          configured# NULL
                        ]
                        # mac_LogicalChannelPriority# 4
                      }
                    ]
                    # rB_Identity# 4 # cn_DomainIdentity# OMIT
                  }
                ]
              }
            ]
          }
        }
      ]
    }

TTCN PDU: CPHY_RL_Setup_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 20
      ],
      ratType: fdd,
      setupMessage:
      {
        physicalChannelInfo:
        [
          dPCHInfo:
          {
            ul_DPCHInfo:
            {
              ul_DPCH_PowerControlInfo:
              [
                fdd:
                {
                  dpcch_PowerOffset: -40,
                  pc_Preamble: 1,
                  sRB_delay: 7,
                  powerControlAlgorithm:
                  [
                    algorithm1: 1
                  ]
                }
              ],
              modeSpecificInfo:
              [
                fdd:
                {
                  scramblingCodeType: longSC,
                  scramblingCode: 0,
                  numberOfDPDCH: OMIT,
                  spreadingFactor: sf64,
                  tfci_Existence: GcTRUE,
                  numberOfFBI_Bits: OMIT,
                  puncturingLimit: pl1
                }
              ]
            },
            dl_DPCHInfo: OMIT
          }
        ]
      }
    }

TTCN PDU: CPHY_TrCH_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 20
      ],
      ratType: fdd,
      trchConfigType:
      [
        dch: Normal
      ],
      configMessage:
      {
        activationTime:
        [
          activateNow: NULL
        ],
        ulconnectedTrCHList:
        [
          {
            trchid: 5,
            ul_TransportChannelType: dch,
            transportChannelInfo:
            {
              tti:
              [
                tti10:
                [
                  {
                    tb_Size: 148,
                    numberOfTbSizeList:
                    [
                      [
                        zero: NULL
                      ],

                      [
                        one: NULL
                      ]
                    ],
                    logicalChannelList:
                    [
                      allSizes: NULL
                    ]
                  }
                ]
              ],
              semistaticTF_Information:
              {
                channelCodingType:
                [
                  convolutional: third
                ],
                rateMatchingAttribute# 192 # crc_Size# crc16
              }
            }
          }
        ]
        # ulTFCS#
        [
          normalTFCI_Signalling#
          [
            complete#
            {
              ctfcSize#
              [
                ctfc2Bit#
                [
                  {
                    ctfc2# 0 # powerOffsetInformation# OMIT
                  }
                  #
                  {
                    ctfc2# 1 # powerOffsetInformation# OMIT
                  }
                ]
              ]
            }
          ]
        ]
        # dlconnectedTrCHList# OMIT# dlTFCS# OMIT
      }
    }

TTCN PDU: CPHY_TrCH_Config_CNF

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 20
      ]
    }

TTCN PDU: CMAC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        physicalChannelIdentity: 20
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          activationTime:
          [
            activateNow: NULL
          ],
          uE_Info:
          {
            u_RNTI: OMIT,
            c_RNTI: OMIT
          },
          trCHInfo:
          {
            ulconnectedTrCHList:
            [
              {
                trchid: 5,
                transportChannelInfo:
                {
                  tti:
                  [
                    tti10:
                    [
                      {
                        tb_Size: 148,
                        numberOfTbSizeList:
                        [
                          [
                            zero: NULL
                          ],

                          [
                            one: NULL
                          ]
                        ],
                        logicalChannelList:
                        [
                          allSizes: NULL
                        ]
                      }
                    ]
                  ],
                  semistaticTF_Information:
                  {
                    channelCodingType:
                    [
                      convolutional: third
                    ],
                    rateMatchingAttribute# 192 # crc_Size# crc16
                  }
                }
              }
            ]
            # ulTFCS#
            [
              normalTFCI_Signalling#
              [
                complete#
                {
                  ctfcSize#
                  [
                    ctfc2Bit#
                    [
                      {
                        ctfc2# 0 # powerOffsetInformation# OMIT
                      }
                      #
                      {
                        ctfc2# 1 # powerOffsetInformation# OMIT
                      }
                    ]
                  ]
                }
              ]
            ]
            # dlconnectedTrCHList# OMIT# dlTFCS# OMIT
          }
          # trCH_LogCHMapping#
          {
            ulconnectedTrCHList#
            [
              {
                trchid# 5 # trCH_LogCHMappingList#
                [
                  {
                    logicalChannel_Mapping#
                    [
                      ul_LogicalChannelMapping#
                      {
                        macHeaderManipulation# normalMacHeader# ul_TransportChannelType# dch# logicalChannelIdentity# 1 # logicalChannelType# dCCH
                      }
                    ]
                    # rB_Identity# 1 # cn_DomainIdentity# OMIT
                  }
                  #
                  {
                    logicalChannel_Mapping#
                    [
                      ul_LogicalChannelMapping#
                      {
                        macHeaderManipulation# normalMacHeader# ul_TransportChannelType# dch# logicalChannelIdentity# 2 # logicalChannelType# dCCH
                      }
                    ]
                    # rB_Identity# 2 # cn_DomainIdentity# OMIT
                  }
                  #
                  {
                    logicalChannel_Mapping#
                    [
                      ul_LogicalChannelMapping#
                      {
                        macHeaderManipulation# normalMacHeader# ul_TransportChannelType# dch# logicalChannelIdentity# 3 # logicalChannelType# dCCH
                      }
                    ]
                    # rB_Identity# 3 # cn_DomainIdentity# OMIT
                  }
                  #
                  {
                    logicalChannel_Mapping#
                    [
                      ul_LogicalChannelMapping#
                      {
                        macHeaderManipulation# normalMacHeader# ul_TransportChannelType# dch# logicalChannelIdentity# 4 # logicalChannelType# dCCH
                      }
                    ]
                    # rB_Identity# 4 # cn_DomainIdentity# OMIT
                  }
                ]
              }
            ]
            # dlconnectedTrCHList# OMIT
          }
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 1
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          sS_rlc_Info:
          {
            sS_ul_RLC_Mode:
            [
              dl_UM_RLC_Mode: NULL
            ],
            sS_dl_RLC_Mode:
            {
              dl_PayloadSize: 136,
              dl_RLCModeInfo:
              [
                ul_UM_RLC_Mode:
                {
                  transmissionRLC_Discard:
                  [
                    timerBasedNoExplicit: dt100
                  ]
                }
              ]
            }
          },
          rB_LogCH_Mapping:
          {
            uLlogicalChannelIdentity: 1,
            dLlogicalChannelIdentity: 1,
            logicalChannelType: OMIT,
            cn_DomainIdentity: OMIT
          }
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 2
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          sS_rlc_Info:
          {
            sS_ul_RLC_Mode:
            [
              dl_AM_RLC_Mode:
              {
                inSequenceDelivery: GcTRUE,
                receivingWindowSize: rw32,
                dl_RLC_StatusInfo:
                {
                  timerStatusProhibit: tsp200,
                  timerEPC: OMIT,
                  missingPDU_Indicator: GcTRUE,
                  timerStatusPeriodic: OMIT
                }
              }
            ],
            sS_dl_RLC_Mode:
            {
              dl_PayloadSize: 128,
              dl_RLCModeInfo:
              [
                ul_AM_RLC_Mode:
                {
                  transmissionRLC_Discard:
                  [
                    noDiscard: dat15
                  ],
                  transmissionWindowSize: tw32,
                  timerRST: tr500,
                  max_RST: rst1,
                  pollingInfo:
                  {
                    timerPollProhibit: tpp200,
                    timerPoll: tp200,
                    poll_PDU: OMIT,
                    poll_SDU: sdu1,
                    lastTransmissionPDU_Poll: GcTRUE,
                    lastRetransmissionPDU_Poll: GcTRUE,
                    pollWindow: pw99,
                    timerPollPeriodic: OMIT
                  }
                }
              ]
            }
          },
          rB_LogCH_Mapping:
          {
            uLlogicalChannelIdentity: 2,
            dLlogicalChannelIdentity: 2,
            logicalChannelType: OMIT,
            cn_DomainIdentity: OMIT
          }
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 3
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          sS_rlc_Info:
          {
            sS_ul_RLC_Mode:
            [
              dl_AM_RLC_Mode:
              {
                inSequenceDelivery: GcTRUE,
                receivingWindowSize: rw32,
                dl_RLC_StatusInfo:
                {
                  timerStatusProhibit: tsp200,
                  timerEPC: OMIT,
                  missingPDU_Indicator: GcTRUE,
                  timerStatusPeriodic: OMIT
                }
              }
            ],
            sS_dl_RLC_Mode:
            {
              dl_PayloadSize: 128,
              dl_RLCModeInfo:
              [
                ul_AM_RLC_Mode:
                {
                  transmissionRLC_Discard:
                  [
                    noDiscard: dat15
                  ],
                  transmissionWindowSize: tw32,
                  timerRST: tr500,
                  max_RST: rst1,
                  pollingInfo:
                  {
                    timerPollProhibit: tpp200,
                    timerPoll: tp200,
                    poll_PDU: OMIT,
                    poll_SDU: sdu1,
                    lastTransmissionPDU_Poll: GcTRUE,
                    lastRetransmissionPDU_Poll: GcTRUE,
                    pollWindow: pw99,
                    timerPollPeriodic: OMIT
                  }
                }
              ]
            }
          },
          rB_LogCH_Mapping:
          {
            uLlogicalChannelIdentity: 3,
            dLlogicalChannelIdentity: 3,
            logicalChannelType: OMIT,
            cn_DomainIdentity: OMIT
          }
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 4
      ],
      ratType: fdd,
      configMessage:
      [
        setup:
        {
          sS_rlc_Info:
          {
            sS_ul_RLC_Mode:
            [
              dl_AM_RLC_Mode:
              {
                inSequenceDelivery: GcTRUE,
                receivingWindowSize: rw32,
                dl_RLC_StatusInfo:
                {
                  timerStatusProhibit: tsp200,
                  timerEPC: OMIT,
                  missingPDU_Indicator: GcTRUE,
                  timerStatusPeriodic: OMIT
                }
              }
            ],
            sS_dl_RLC_Mode:
            {
              dl_PayloadSize: 128,
              dl_RLCModeInfo:
              [
                ul_AM_RLC_Mode:
                {
                  transmissionRLC_Discard:
                  [
                    noDiscard: dat15
                  ],
                  transmissionWindowSize: tw32,
                  timerRST: tr500,
                  max_RST: rst1,
                  pollingInfo:
                  {
                    timerPollProhibit: tpp200,
                    timerPoll: tp200,
                    poll_PDU: OMIT,
                    poll_SDU: sdu1,
                    lastTransmissionPDU_Poll: GcTRUE,
                    lastRetransmissionPDU_Poll: GcTRUE,
                    pollWindow: pw99,
                    timerPollPeriodic: OMIT
                  }
                }
              ]
            }
          },
          rB_LogCH_Mapping:
          {
            uLlogicalChannelIdentity: 4,
            dLlogicalChannelIdentity: 4,
            logicalChannelType: OMIT,
            cn_DomainIdentity: OMIT
          }
        }
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 1
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 2
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 3
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        rB_Identity: 4
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CMAC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        physicalChannelIdentity: 26
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CMAC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: -1,
      routingInfo:
      [
        physicalChannelIdentity: 20
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CPHY_TrCH_Release_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 26
      ],
      trchConfigType:
      [
        dch: Normal
      ]
    }

TTCN PDU: CPHY_TrCH_Release_CNF

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 26
      ]
    }

TTCN PDU: CPHY_TrCH_Release_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 20
      ],
      trchConfigType:
      [
        dch: Normal
      ]
    }

TTCN PDU: CPHY_TrCH_Release_CNF

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 20
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: 0
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CMAC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 8
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CPHY_TrCH_Release_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 8
      ],
      trchConfigType:
      [
        nonDch: NULL
      ]
    }

TTCN PDU: CPHY_TrCH_Release_CNF

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 8
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -2
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CMAC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 5
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CPHY_TrCH_Release_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 5
      ],
      trchConfigType:
      [
        nonDch: NULL
      ]
    }

TTCN PDU: CPHY_TrCH_Release_CNF

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 5
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CMAC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 4
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CPHY_TrCH_Release_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 4
      ],
      trchConfigType:
      [
        nonDch: NULL
      ]
    }

TTCN PDU: CPHY_TrCH_Release_CNF

(To search, click here and then press Ctrl+F)

    {
      cellId: 0,
      routingInfo:
      [
        physicalChannelIdentity: 4
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: 0
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CMAC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        physicalChannelIdentity: 8
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CPHY_TrCH_Release_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        physicalChannelIdentity: 8
      ],
      trchConfigType:
      [
        nonDch: NULL
      ]
    }

TTCN PDU: CPHY_TrCH_Release_CNF

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        physicalChannelIdentity: 8
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -2
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CMAC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        physicalChannelIdentity: 5
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CPHY_TrCH_Release_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        physicalChannelIdentity: 5
      ],
      trchConfigType:
      [
        nonDch: NULL
      ]
    }

TTCN PDU: CPHY_TrCH_Release_CNF

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        physicalChannelIdentity: 5
      ]
    }

TTCN PDU: CRLC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        rB_Identity: -1
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CMAC_Config_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        physicalChannelIdentity: 4
      ],
      ratType: fdd,
      configMessage:
      [
        release: NULL
      ]
    }

TTCN PDU: CPHY_TrCH_Release_REQ

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        physicalChannelIdentity: 4
      ],
      trchConfigType:
      [
        nonDch: NULL
      ]
    }

TTCN PDU: CPHY_TrCH_Release_CNF

(To search, click here and then press Ctrl+F)

    {
      cellId: 3,
      routingInfo:
      [
        physicalChannelIdentity: 4
      ]
    }