|  |  | RRC_wk26-RRC_Measurements-tc_8_4_1_25 | Contains 7873 lines/items
| StartTimer:[1] t_Guard [300] 300 s Attach:[3] Enter Test Step tc_8_4_1_25::lt_InitVariables( )
| Attach:[35] Enter Test Step ts_RRC_InitVariables( cell_DCH )
| Attach:[1] Enter Test Step ts_AssignCN_Domain( )
| Assignment:[2] tcv_CN_Domain := cs_domain Attach:[1] Exit Test Step ts_AssignCN_Domain
Attach:[3] Enter Test Step ts_RRC_InitVariablesCS( )
| Attach:[1] Enter Test Step ts_InitVariables( )
| Attach:[1] Enter Test Step ts_InitVariables::lt_CalculateFrequencyInfo( )
| Attach:[10] Enter Test Step ts_InitVariables::lt_CalculateFreqMid( )
| Attach:[13] Enter Test Step ts_InitVariables::lt_CheckFreqSeperation( 10700 )
| Assignment:[30] tcv_Res := GcTRUE Attach:[13] Exit Test Step ts_InitVariables::lt_CheckFreqSeperation
Assignment:[17] tcv_FreqInfoMid := { modeSpecificInfo: [fdd: { uarfcn_UL: OMIT, uarfcn_DL: 10700 } ]} Attach:[10] Exit Test Step ts_InitVariables::lt_CalculateFreqMid
Attach:[11] Enter Test Step ts_InitVariables::lt_CalculateFreqHigh( )
| Attach:[18] Enter Test Step ts_InitVariables::lt_CheckFreqSeperation( 10837 )
| Assignment:[30] tcv_Res := GcTRUE Attach:[18] Exit Test Step ts_InitVariables::lt_CheckFreqSeperation
Assignment:[22] tcv_FreqInfoHigh := { modeSpecificInfo: [fdd: { uarfcn_UL: OMIT, uarfcn_DL: 10837 } ]} Attach:[11] Exit Test Step ts_InitVariables::lt_CalculateFreqHigh
Attach:[12] Enter Test Step ts_InitVariables::lt_CalculateFreqLow( )
| Attach:[23] Enter Test Step ts_InitVariables::lt_CheckFreqSeperation( 10563 )
| Assignment:[30] tcv_Res := GcTRUE Attach:[23] Exit Test Step ts_InitVariables::lt_CheckFreqSeperation
Assignment:[27] tcv_FreqInfoLow := { modeSpecificInfo: [fdd: { uarfcn_UL: OMIT, uarfcn_DL: 10563 } ]} Attach:[12] Exit Test Step ts_InitVariables::lt_CalculateFreqLow
Attach:[1] Exit Test Step ts_InitVariables::lt_CalculateFrequencyInfo
Attach:[2] Enter Test Step ts_InitVariables::lt_Init_SSInfo_CellA( )
| Assignment:[48] tcv_CellInfoA := (view Assignment) Attach:[2] Exit Test Step ts_InitVariables::lt_Init_SSInfo_CellA
Attach:[3] Enter Test Step ts_InitVariables::lt_Init_SSInfo_CellB( )
| Assignment:[49] tcv_CellInfoB := (view Assignment) Attach:[3] Exit Test Step ts_InitVariables::lt_Init_SSInfo_CellB
Attach:[4] Enter Test Step ts_InitVariables::lt_Init_SSInfo_CellC( )
| Assignment:[50] tcv_CellInfoC := (view Assignment) Attach:[4] Exit Test Step ts_InitVariables::lt_Init_SSInfo_CellC
Attach:[5] Enter Test Step ts_InitVariables::lt_Init_SSInfo_CellD( )
| Assignment:[51] tcv_CellInfoD := (view Assignment) Attach:[5] Exit Test Step ts_InitVariables::lt_Init_SSInfo_CellD
Attach:[6] Enter Test Step ts_InitVariables::lt_Init_SSInfo_CellE( )
| Assignment:[52] tcv_CellInfoE := (view Assignment) Attach:[6] Exit Test Step ts_InitVariables::lt_Init_SSInfo_CellE
Attach:[7] Enter Test Step ts_InitVariables::lt_Init_SSInfo_CellF( )
| Assignment:[53] tcv_CellInfoF := (view Assignment) Attach:[7] Exit Test Step ts_InitVariables::lt_Init_SSInfo_CellF
Attach:[8] Enter Test Step ts_InitVariables::lt_Init_SSInfo_CellG( )
| Assignment:[54] tcv_CellInfoG := (view Assignment) Attach:[8] Exit Test Step ts_InitVariables::lt_Init_SSInfo_CellG
Attach:[9] Enter Test Step ts_InitVariables::lt_Init_SSInfo_CellH( )
| Assignment:[55] tcv_CellInfoH := (view Assignment) Attach:[9] Exit Test Step ts_InitVariables::lt_Init_SSInfo_CellH
Attach:[1] Exit Test Step ts_InitVariables
Assignment:[2] tcv_CN_Domain := cs_domain Assignment:[2] tcv_RAB_Id := '00000001'B Attach:[3] Enter Test Step ts_RRC_InitVariablesCS::lt_RRC_InitServVarCS( )
| Assignment:[5] tcv_RRC_RAB_Type := cell_DCH_Speech Assignment:[5] tcv_RRC_PagingCau := terminatingConversationalCall Assignment:[5] tcv_RRC_EstCauMO := originatingConversationalCall Assignment:[5] tcv_RRC_EstCauMT := terminatingConversationalCall Attach:[3] Exit Test Step ts_RRC_InitVariablesCS::lt_RRC_InitServVarCS
Attach:[3] Exit Test Step ts_RRC_InitVariablesCS
Attach:[35] Exit Test Step ts_RRC_InitVariables
Assignment:[36] tcv_CellInfoA := (view Assignment) Assignment:[37] tcv_CellInfoD := (view Assignment) Assignment:[38] powerpCPICH := -55 Assignment:[39] attenuationLevel := 30 Assignment:[40] attenuationLevel := 0 Attach:[3] Exit Test Step tc_8_4_1_25::lt_InitVariables
Attach:[4] Enter Test Step ts_SS_CreateCellDCH( 0 )
| Attach:[1] Enter Test Step ts_SS_CellCfg( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[4] Enter Test Step ts_SS_CellCfg::lt_CelllsAlreadyStarted( 0 )
| Attach:[11] Enter Test Step ts_CountConfiguredCell( )
| Assignment:[1] tcv_NumCfgCell := 0 Attach:[2] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 0 , frequenc ...
| (view Test Step parameters) Attach:[2] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[3] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 1 , frequenc ...
| (view Test Step parameters) Attach:[3] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[4] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 2 , frequenc ...
| (view Test Step parameters) Attach:[4] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[5] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 3 , frequenc ...
| (view Test Step parameters) Attach:[5] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[6] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 4 , frequenc ...
| (view Test Step parameters) Attach:[6] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[7] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 5 , frequenc ...
| (view Test Step parameters) Attach:[7] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[8] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 6 , frequenc ...
| (view Test Step parameters) Attach:[8] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[9] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 7 , frequenc ...
| (view Test Step parameters) Attach:[9] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[11] Exit Test Step ts_CountConfiguredCell
Attach:[13] Enter Test Step ts_MM_PwrOrUSIM_Off( GcTRUE )
| Attach:[4] Enter Test Step ts_MMI_UE_SwitchOff( )
| 00:00:05.190 - Primitive: MMI_CmdReq Send event:[1] Ut ! MMI_CmdReq = PDU: { cmd: "Please switch off the UE" } 00:00:08.930 - Primitive: MMI_CmdCnf begin "ca_MMI_CmdCnf" of type MMI_CmdCnf (SEQUENCE) [UNIVERSAL 16] begin "result" of type BOOLEAN [UNIVERSAL 1] matching GcTRUE against GcTRUE end "result" of type BOOLEAN end "ca_MMI_CmdCnf" of type MMI_CmdCnf Receive event:[2] Ut ? MMI_CmdCnf = PDU: { result: GcTRUE , resultString: OMIT} Attach:[4] Exit Test Step ts_MMI_UE_SwitchOff
Attach:[13] Exit Test Step ts_MM_PwrOrUSIM_Off
00:00:08.930 - Primitive: CPHY_Ini_REQ Send event:[15] CPHY ! CPHY_Ini_REQ = PDU: defaultRadioEnvironment 00:00:10.190 - Primitive: CPHY_Ini_CNF begin "car_IniCnf" of type CPHY_Ini_CNF (SEQUENCE) [UNIVERSAL 16] begin "confirmation" of type NULL [UNIVERSAL 5] matching NULL against NULL end "confirmation" of type NULL end "car_IniCnf" of type CPHY_Ini_CNF Receive event:[16] CPHY ? CPHY_Ini_CNF = PDU: { confirmation: NULL} Assignment:[17] tCell := 0 Attach:[4] Exit Test Step ts_SS_CellCfg::lt_CelllsAlreadyStarted
00:00:10.190 - Primitive: CPHY_Cell_Config_REQ Send event:[6] CPHY ! CPHY_Cell_Config_REQ = PDU (view PDU) 00:00:10.330 - Primitive: CPHY_Cell_Config_CNF begin "ca_CellCfgCnf" of type CPHY_Cell_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER end "ca_CellCfgCnf" of type CPHY_Cell_Config_CNF Receive event:[7] CPHY ? CPHY_Cell_Config_CNF = PDU: { cellId: 0 } Attach:[8] Enter Test Step ts_SaveCellInfo( 0 )
| Assignment:[2] tcv_CellInfoA := (view Assignment) Attach:[8] Exit Test Step ts_SaveCellInfo
Attach:[1] Exit Test Step ts_SS_CellCfg
Attach:[2] Enter Test Step ts_SS_BCH_SCH_CPICH_Cfg( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
00:00:10.330 - Primitive: CPHY_RL_Setup_REQ Send event:[3] CPHY ! CPHY_RL_Setup_REQ = PDU (view PDU) 00:00:10.440 - Primitive: CPHY_RL_Setup_CNF begin "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF Receive event:[4] CPHY ? CPHY_RL_Setup_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 0 ]} 00:00:10.440 - Primitive: CPHY_RL_Setup_REQ Send event:[5] CPHY ! CPHY_RL_Setup_REQ = PDU (view PDU) 00:00:10.490 - Primitive: CPHY_RL_Setup_CNF begin "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF Receive event:[6] CPHY ? CPHY_RL_Setup_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 1 ]} 00:00:10.490 - Primitive: CPHY_RL_Setup_REQ Send event:[7] CPHY ! CPHY_RL_Setup_REQ = PDU (view PDU) 00:00:10.630 - Primitive: CPHY_RL_Setup_CNF begin "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF Receive event:[8] CPHY ? CPHY_RL_Setup_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 2 ]} 00:00:10.630 - Primitive: CPHY_RL_Setup_REQ Send event:[9] CPHY ! CPHY_RL_Setup_REQ = PDU (view PDU) 00:00:10.800 - Primitive: CPHY_RL_Setup_CNF begin "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF Receive event:[10] CPHY ? CPHY_RL_Setup_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 4 ]} 00:00:10.800 - Primitive: CPHY_TrCH_Config_REQ Send event:[11] CPHY ! CPHY_TrCH_Config_REQ = PDU (view PDU) 00:00:10.830 - Primitive: CPHY_TrCH_Config_CNF begin "ca_TrChCfgCnf" of type CPHY_TrCH_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_TrChCfgCnf" of type CPHY_TrCH_Config_CNF Receive event:[12] CPHY ? CPHY_TrCH_Config_CNF = PDU (view PDU) 00:00:10.830 - Primitive: CMAC_Config_REQ Send event:[13] CMAC ! CMAC_Config_REQ = PDU (view PDU) 00:00:10.860 - Primitive: CMAC_Config_CNF begin "ca_CMAC_CfgCnf" of type CMAC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_CfgCnf" of type CMAC_Config_CNF Receive event:[14] CMAC ? CMAC_Config_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 4 ]} Attach:[2] Exit Test Step ts_SS_BCH_SCH_CPICH_Cfg
Attach:[3] Enter Test Step ts_SS_PCH_FACH_CCCH_Cfg( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
00:00:10.860 - Primitive: CPHY_RL_Setup_REQ Send event:[3] CPHY ! CPHY_RL_Setup_REQ = PDU (view PDU) 00:00:10.970 - Primitive: CPHY_RL_Setup_CNF begin "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 5 against 5 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF Receive event:[4] CPHY ? CPHY_RL_Setup_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 5 ]} 00:00:10.970 - Primitive: CPHY_TrCH_Config_REQ Send event:[5] CPHY ! CPHY_TrCH_Config_REQ = PDU (view PDU) 00:00:11.000 - Primitive: CPHY_TrCH_Config_CNF begin "ca_TrChCfgCnf" of type CPHY_TrCH_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 5 against 5 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_TrChCfgCnf" of type CPHY_TrCH_Config_CNF Receive event:[6] CPHY ? CPHY_TrCH_Config_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 5 ]} 00:00:11.000 - Primitive: CMAC_Config_REQ Send event:[7] CMAC ! CMAC_Config_REQ = PDU (view PDU) 00:00:11.020 - Primitive: CMAC_Config_CNF begin "ca_CMAC_CfgCnf" of type CMAC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 5 against 5 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_CfgCnf" of type CMAC_Config_CNF Receive event:[8] CMAC ? CMAC_Config_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 5 ]} 00:00:11.020 - Primitive: CPHY_RL_Setup_REQ Send event:[9] CPHY ! CPHY_RL_Setup_REQ = PDU (view PDU) 00:00:11.080 - Primitive: CPHY_RL_Setup_CNF begin "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF Receive event:[10] CPHY ? CPHY_RL_Setup_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 6 ]} Attach:[3] Exit Test Step ts_SS_PCH_FACH_CCCH_Cfg
Attach:[4] Enter Test Step ts_SS_RACH_CCCH_Cfg( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
00:00:11.080 - Primitive: CPHY_RL_Setup_REQ Send event:[3] CPHY ! CPHY_RL_Setup_REQ = PDU (view PDU) 00:00:11.130 - Primitive: CPHY_RL_Setup_CNF begin "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 7 against 7 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF Receive event:[4] CPHY ? CPHY_RL_Setup_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 7 ]} 00:00:11.130 - Primitive: CPHY_RL_Setup_REQ Send event:[5] CPHY ! CPHY_RL_Setup_REQ = PDU (view PDU) 00:00:11.140 - Primitive: CPHY_RL_Setup_CNF begin "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 8 against 8 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF Receive event:[6] CPHY ? CPHY_RL_Setup_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 8 ]} 00:00:11.140 - Primitive: CPHY_TrCH_Config_REQ Send event:[7] CPHY ! CPHY_TrCH_Config_REQ = PDU (view PDU) 00:00:11.350 - Primitive: CPHY_TrCH_Config_CNF begin "ca_TrChCfgCnf" of type CPHY_TrCH_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 8 against 8 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_TrChCfgCnf" of type CPHY_TrCH_Config_CNF Receive event:[8] CPHY ? CPHY_TrCH_Config_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 8 ]} 00:00:11.350 - Primitive: CMAC_Config_REQ Send event:[9] CMAC ! CMAC_Config_REQ = PDU (view PDU) 00:00:11.380 - Primitive: CMAC_Config_CNF begin "ca_CMAC_CfgCnf" of type CMAC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 8 against 8 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_CfgCnf" of type CMAC_Config_CNF Receive event:[10] CMAC ? CMAC_Config_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 8 ]} Attach:[4] Exit Test Step ts_SS_RACH_CCCH_Cfg
Attach:[5] Enter Test Step ts_CountConfiguredCell( )
| Assignment:[1] tcv_NumCfgCell := 0 Attach:[2] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 0 , frequenc ...
| (view Test Step parameters) Attach:[2] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[3] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 1 , frequenc ...
| (view Test Step parameters) Attach:[3] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[4] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 2 , frequenc ...
| (view Test Step parameters) Attach:[4] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[5] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 3 , frequenc ...
| (view Test Step parameters) Attach:[5] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[6] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 4 , frequenc ...
| (view Test Step parameters) Attach:[6] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[7] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 5 , frequenc ...
| (view Test Step parameters) Attach:[7] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[8] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 6 , frequenc ...
| (view Test Step parameters) Attach:[8] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[9] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 7 , frequenc ...
| (view Test Step parameters) Attach:[9] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[5] Exit Test Step ts_CountConfiguredCell
Attach:[7] Enter Test Step ts_SS_1DCH_DCCH_Cfg( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Assignment:[3] tcv_TGCFN := 0 00:00:11.380 - Primitive: CPHY_RL_Setup_REQ Send event:[4] CPHY ! CPHY_RL_Setup_REQ = PDU (view PDU) 00:00:11.440 - Primitive: CPHY_RL_Setup_CNF begin "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 26 against 26 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF Receive event:[5] CPHY ? CPHY_RL_Setup_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 26 ]} 00:00:11.440 - Primitive: CPHY_TrCH_Config_REQ Send event:[6] CPHY ! CPHY_TrCH_Config_REQ = PDU (view PDU) 00:00:11.470 - Primitive: CPHY_TrCH_Config_CNF begin "ca_TrChCfgCnf" of type CPHY_TrCH_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 26 against 26 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_TrChCfgCnf" of type CPHY_TrCH_Config_CNF Receive event:[7] CPHY ? CPHY_TrCH_Config_CNF = PDU (view PDU) 00:00:11.470 - Primitive: CMAC_Config_REQ Send event:[8] CMAC ! CMAC_Config_REQ = PDU (view PDU) 00:00:11.500 - Primitive: CMAC_Config_CNF begin "ca_CMAC_CfgCnf" of type CMAC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 26 against 26 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_CfgCnf" of type CMAC_Config_CNF Receive event:[9] CMAC ? CMAC_Config_CNF = PDU: { cellId: -1 , routingInfo: [physicalChannelIdentity: 26 ]} 00:00:11.500 - Primitive: CPHY_RL_Setup_REQ Send event:[10] CPHY ! CPHY_RL_Setup_REQ = PDU (view PDU) 00:00:11.520 - Primitive: CPHY_RL_Setup_CNF begin "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 20 against 20 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF Receive event:[11] CPHY ? CPHY_RL_Setup_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 20 ]} 00:00:11.520 - Primitive: CPHY_TrCH_Config_REQ Send event:[12] CPHY ! CPHY_TrCH_Config_REQ = PDU (view PDU) 00:00:11.660 - Primitive: CPHY_TrCH_Config_CNF begin "ca_TrChCfgCnf" of type CPHY_TrCH_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 20 against 20 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_TrChCfgCnf" of type CPHY_TrCH_Config_CNF Receive event:[13] CPHY ? CPHY_TrCH_Config_CNF = PDU (view PDU) 00:00:11.660 - Primitive: CMAC_Config_REQ Send event:[14] CMAC ! CMAC_Config_REQ = PDU (view PDU) 00:00:11.690 - Primitive: CMAC_Config_CNF begin "ca_CMAC_CfgCnf" of type CMAC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 20 against 20 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_CfgCnf" of type CMAC_Config_CNF Receive event:[15] CMAC ? CMAC_Config_CNF = PDU: { cellId: -1 , routingInfo: [physicalChannelIdentity: 20 ]} Attach:[7] Exit Test Step ts_SS_1DCH_DCCH_Cfg
Attach:[8] Enter Test Step ts_SS_RB_BCCH_BCH_Cfg( 0 )
| 00:00:11.690 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:00:12.300 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} Attach:[8] Exit Test Step ts_SS_RB_BCCH_BCH_Cfg
Attach:[9] Enter Test Step ts_SS_RB_PCCH_Cfg( 0 )
| 00:00:12.300 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:00:12.360 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -2 against -2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -2 ]} Attach:[9] Exit Test Step ts_SS_RB_PCCH_Cfg
Attach:[10] Enter Test Step ts_SS_RB0_Cfg( 0 )
| 00:00:12.360 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:00:12.410 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: 0 ]} 00:00:12.410 - Primitive: CRLC_Config_REQ Send event:[3] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:00:12.580 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[4] CRLC ? CRLC_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: 0 ]} Attach:[10] Exit Test Step ts_SS_RB0_Cfg
Attach:[11] Enter Test Step ts_SS_RB1_ToRB4_Cfg( )
| 00:00:12.580 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:00:12.720 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 1 ]} 00:00:12.720 - Primitive: CRLC_Config_REQ Send event:[3] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:00:12.790 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[4] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 2 ]} 00:00:12.790 - Primitive: CRLC_Config_REQ Send event:[5] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:00:12.890 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[6] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 3 ]} 00:00:12.890 - Primitive: CRLC_Config_REQ Send event:[7] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:00:13.040 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[8] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 4 ]} Attach:[11] Exit Test Step ts_SS_RB1_ToRB4_Cfg
Assignment:[12] DL_DPCH_SHO := GcTRUE Assignment:[12] UL_DPCH_SHO := GcTRUE Assignment:[12] cellConfig := cell_DCH_StandAloneSRB_NoConn Attach:[13] Enter Test Step ts_SaveCellInfo( 0 )
| Assignment:[2] tcv_CellInfoA := (view Assignment) Attach:[13] Exit Test Step ts_SaveCellInfo
Attach:[4] Exit Test Step ts_SS_CreateCellDCH
Attach:[5] Enter Test Step ts_SendDef_sysInfo_MultiCell( 0 )
| Attach:[1] Enter Test Step ts_InitializeSIB11_SIB12( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[3] Enter Test Step ts_InitializeSIB11_SIB12::lt_1Or2PLMN( 0 )
| Assignment:[10] tcv_SIB11 := (view Assignment) Assignment:[10] tcv_SIB12 := (view Assignment) Attach:[3] Exit Test Step ts_InitializeSIB11_SIB12::lt_1Or2PLMN
Attach:[1] Exit Test Step ts_InitializeSIB11_SIB12
Attach:[2] Enter Test Step ts_InitMIB_SB1( 0 )
| Assignment:[2] tcv_MIB := (view Assignment) Assignment:[2] tcv_SB1 := (view Assignment) Attach:[2] Exit Test Step ts_InitMIB_SB1
Attach:[3] Enter Test Step ts_SendDefSysInfo_LongNeighCellInfo( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[2] Enter Test Step ts_UTRAN_GERAN_ParaInit( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Assignment:[3] tcv_SIB3 := (view Assignment) Assignment:[3] tcv_SIB4 := (view Assignment) Attach:[2] Exit Test Step ts_UTRAN_GERAN_ParaInit
Attach:[3] Enter Test Step ts_CellDependentPara( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Assignment:[3] cellIdentity := '0000000000000000000000000000'B Assignment:[3] cellIdentity := '0000000000000000000000000000'B Attach:[3] Exit Test Step ts_CellDependentPara
Attach:[4] Enter Test Step ts_InitializeSIB2AndSIB18( { cellId: 0 , frequenc ...
| (view Test Step parameters) Assignment:[1] tcv_SIB2 := { ura_IdentityList: [ '0000000000000001'B ] , nonCriticalExtensions: OMIT} Assignment:[3] tcv_SIB18 := (view Assignment) Attach:[4] Exit Test Step ts_InitializeSIB2AndSIB18
Assignment:[5] tcv_MIB := (view Assignment) Assignment:[5] tcv_SB1 := (view Assignment) Attach:[7] Enter Test Step ts_SendSIB1_LongNeighCellInfo( { cn_CommonGSM_MAP_NAS ...
| (view Test Step parameters) Assignment:[1] tcv_SIB1 := (view Assignment) Assignment:[1] seg1 := (view Assignment) Assignment:[1] seg2 := '00000000000000000001'B Attach:[4] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:13.050 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[4] Exit Test Step ts_Scheduling
00:00:13.070 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[5] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} 00:00:13.070 - Primitive: RLC_TR_DATA_REQ 00:00:13.080 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[6] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Assignment:[7] sysInfoType1 := 2 Attach:[8] Enter Test Step ts_ChangeMIB_ValueTag( )
| Attach:[8] Exit Test Step ts_ChangeMIB_ValueTag
Attach:[7] Exit Test Step ts_SendSIB1_LongNeighCellInfo
Attach:[8] Enter Test Step ts_SendSIB2_LongNeighCellInfo( { ura_IdentityList: [ ...
| (view Test Step parameters) Assignment:[1] tcv_SIB2 := { ura_IdentityList: [ '0000000000000001'B ] , nonCriticalExtensions: OMIT} Assignment:[1] seg1 := '00000000000000000001'B Assignment:[1] seg2 := (view Assignment) Attach:[4] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:13.100 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[4] Exit Test Step ts_Scheduling
00:00:13.110 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[5] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} 00:00:13.110 - Primitive: RLC_TR_DATA_REQ 00:00:13.110 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[6] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Assignment:[7] sysInfoType2 := 2 Attach:[8] Enter Test Step ts_ChangeMIB_ValueTag( )
| Attach:[8] Exit Test Step ts_ChangeMIB_ValueTag
Attach:[8] Exit Test Step ts_SendSIB2_LongNeighCellInfo
Attach:[9] Enter Test Step ts_SendSIB3_LongNeighCellInfo( { sib4indicator: GcTRU ...
| (view Test Step parameters) Assignment:[1] tcv_SIB3 := (view Assignment) Assignment:[1] seg1 := (view Assignment) Assignment:[1] seg2 := '100000101000000010000001'B Attach:[4] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:13.110 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[4] Exit Test Step ts_Scheduling
00:00:13.130 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[5] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} 00:00:13.130 - Primitive: RLC_TR_DATA_REQ 00:00:13.130 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[6] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Assignment:[7] sysInfoType3 := 2 Attach:[8] Enter Test Step ts_ChangeMIB_ValueTag( )
| Attach:[8] Exit Test Step ts_ChangeMIB_ValueTag
Attach:[9] Exit Test Step ts_SendSIB3_LongNeighCellInfo
Attach:[10] Enter Test Step ts_SendSIB4_LongNeighCellInfo( { cellIdentity: '00000 ...
| (view Test Step parameters) Assignment:[1] tcv_SIB4 := (view Assignment) Assignment:[1] seg1 := (view Assignment) Assignment:[1] seg2 := '100000101000000010000001'B Attach:[4] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:13.130 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[4] Exit Test Step ts_Scheduling
00:00:13.140 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[5] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} 00:00:13.140 - Primitive: RLC_TR_DATA_REQ 00:00:13.140 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[6] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Assignment:[7] sysInfoType4 := 2 Attach:[8] Enter Test Step ts_ChangeMIB_ValueTag( )
| Attach:[8] Exit Test Step ts_ChangeMIB_ValueTag
Attach:[10] Exit Test Step ts_SendSIB4_LongNeighCellInfo
Attach:[11] Enter Test Step ts_SendSIB5_LongNeighCellInfo( { sib6indicator: GcTRU ...
| (view Test Step parameters) Assignment:[1] tcv_Segs := (view Assignment) Assignment:[38] sysInfoType5 := 2 Assignment:[38] scheduling := (view Assignment) Attach:[39] Enter Test Step ts_ChangeMIB_ValueTag( )
| Attach:[39] Exit Test Step ts_ChangeMIB_ValueTag
Attach:[40] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:13.180 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[40] Exit Test Step ts_Scheduling
00:00:13.190 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[41] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} 00:00:13.190 - Primitive: RLC_TR_DATA_REQ 00:00:13.190 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[42] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[43] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:13.190 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[43] Exit Test Step ts_Scheduling
00:00:13.210 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[44] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} 00:00:13.210 - Primitive: RLC_TR_DATA_REQ 00:00:13.210 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[45] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[46] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:13.210 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[46] Exit Test Step ts_Scheduling
00:00:13.220 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[47] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} 00:00:13.220 - Primitive: RLC_TR_DATA_REQ 00:00:13.220 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[48] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[49] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:13.220 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[49] Exit Test Step ts_Scheduling
00:00:13.240 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[50] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} 00:00:13.240 - Primitive: RLC_TR_DATA_REQ 00:00:13.240 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[52] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[11] Exit Test Step ts_SendSIB5_LongNeighCellInfo
Attach:[12] Enter Test Step ts_SendSIB6_LongNeighCellInfo( { pich_PowerOffset: -5 ...
| (view Test Step parameters) Assignment:[1] tcv_Segs := (view Assignment) Assignment:[5] sysInfoType6 := 2 Assignment:[5] scheduling := { scheduling: { segCount: OMIT, sib_Pos: [rep64: 2 ], sib_PosOffsetInfo: OMIT} } Attach:[6] Enter Test Step ts_ChangeSB1_ValueTag( )
| Assignment:[2] tcv_SB1_ValueTag := 2 Assignment:[2] sysInfoTypeSB1 := 2 Assignment:[2] tcv_SB1_ValueTagChanged := GcTRUE Attach:[3] Enter Test Step ts_ChangeMIB_ValueTag( )
| Attach:[3] Exit Test Step ts_ChangeMIB_ValueTag
Attach:[6] Exit Test Step ts_ChangeSB1_ValueTag
Attach:[7] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:13.240 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[7] Exit Test Step ts_Scheduling
00:00:13.250 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[8] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} Attach:[9] Enter Test Step ts_SendSIB6_LongNeighCellInfo::lt_CompleteSIB( systemInformationBlockType6 )
| 00:00:13.250 - Primitive: RLC_TR_DATA_REQ 00:00:13.250 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[76] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[9] Exit Test Step ts_SendSIB6_LongNeighCellInfo::lt_CompleteSIB
Attach:[10] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:13.250 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[10] Exit Test Step ts_Scheduling
00:00:13.270 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[11] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} 00:00:13.270 - Primitive: RLC_TR_DATA_REQ 00:00:13.270 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[12] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[13] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:13.270 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[13] Exit Test Step ts_Scheduling
00:00:13.290 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[14] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} 00:00:13.290 - Primitive: RLC_TR_DATA_REQ 00:00:13.290 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[15] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[16] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:13.290 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[16] Exit Test Step ts_Scheduling
00:00:13.300 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[17] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} 00:00:13.300 - Primitive: RLC_TR_DATA_REQ 00:00:13.300 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[18] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[12] Exit Test Step ts_SendSIB6_LongNeighCellInfo
Attach:[13] Enter Test Step ts_SendSIB7_LongNeighCellInfo( { modeSpecificInfo: [f ...
| (view Test Step parameters) Assignment:[1] tcv_Segs := (view Assignment) Assignment:[1] tcv_SIB7 := (view Assignment) Assignment:[1] tcv_Segs_SIB12 := (view Assignment) Attach:[4] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:13.300 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[4] Exit Test Step ts_Scheduling
00:00:13.320 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[5] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} Attach:[6] Enter Test Step ts_SendSIB7_LongNeighCellInfo::lt_CompleteSIB7OrLastSIB12_CompleteSIB7( { modeSpecificInfo: [f ...
| (view Test Step parameters) 00:00:13.320 - Primitive: RLC_TR_DATA_REQ 00:00:13.320 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[36] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[6] Exit Test Step ts_SendSIB7_LongNeighCellInfo::lt_CompleteSIB7OrLastSIB12_CompleteSIB7
Attach:[7] Enter Test Step ts_SendSIB7_LongNeighCellInfo::lt_ConcatWithSIB3( { modeSpecificInfo: [f ...
| (view Test Step parameters) Assignment:[10] seg2 := (view Assignment) Attach:[13] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:13.320 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[13] Exit Test Step ts_Scheduling
00:00:13.330 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[14] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} 00:00:13.330 - Primitive: RLC_TR_DATA_REQ 00:00:13.330 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[15] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[7] Exit Test Step ts_SendSIB7_LongNeighCellInfo::lt_ConcatWithSIB3
Attach:[8] Enter Test Step ts_SendSIB7_LongNeighCellInfo::lt_ConcatWithSIB18( { modeSpecificInfo: [f ...
| (view Test Step parameters) Assignment:[16] seg2 := '100000'B Attach:[19] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:13.330 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[19] Exit Test Step ts_Scheduling
00:00:13.350 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[20] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} 00:00:13.350 - Primitive: RLC_TR_DATA_REQ 00:00:13.350 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[21] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[8] Exit Test Step ts_SendSIB7_LongNeighCellInfo::lt_ConcatWithSIB18
Attach:[9] Enter Test Step ts_SendSIB7_LongNeighCellInfo::lt_ConcatWithSIB4( { modeSpecificInfo: [f ...
| (view Test Step parameters) Assignment:[22] seg2 := (view Assignment) Attach:[25] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:13.350 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[25] Exit Test Step ts_Scheduling
00:00:13.360 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[26] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} 00:00:13.360 - Primitive: RLC_TR_DATA_REQ 00:00:13.360 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[27] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[9] Exit Test Step ts_SendSIB7_LongNeighCellInfo::lt_ConcatWithSIB4
Attach:[13] Exit Test Step ts_SendSIB7_LongNeighCellInfo
Attach:[14] Enter Test Step ts_SendSIB11_LongNeighCellInfo( { sib12indicator: GcTR ...
| (view Test Step parameters) Assignment:[1] tcv_Segs := (view Assignment) Assignment:[20] sysInfoType11 := 2 Assignment:[20] scheduling := (view Assignment) Attach:[21] Enter Test Step ts_ChangeSB1_ValueTag( )
| Attach:[21] Exit Test Step ts_ChangeSB1_ValueTag
Attach:[22] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:13.390 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[22] Exit Test Step ts_Scheduling
00:00:13.410 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[23] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} 00:00:13.410 - Primitive: RLC_TR_DATA_REQ 00:00:13.410 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[24] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[25] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:13.410 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[25] Exit Test Step ts_Scheduling
00:00:13.430 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[26] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} 00:00:13.430 - Primitive: RLC_TR_DATA_REQ 00:00:13.430 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[27] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[28] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:13.430 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[28] Exit Test Step ts_Scheduling
00:00:13.440 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[29] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} 00:00:13.440 - Primitive: RLC_TR_DATA_REQ 00:00:13.440 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[30] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[31] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:13.440 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[31] Exit Test Step ts_Scheduling
00:00:13.460 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[32] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} 00:00:13.460 - Primitive: RLC_TR_DATA_REQ 00:00:13.460 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[34] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[14] Exit Test Step ts_SendSIB11_LongNeighCellInfo
Attach:[15] Enter Test Step ts_SendSIB12_LongNeighCellInfo( { fach_MeasurementOcca ...
| (view Test Step parameters) Assignment:[1] tcv_Segs_SIB12 := (view Assignment) Assignment:[5] sysInfoType12 := 2 Assignment:[5] scheduling := { scheduling: { segCount: OMIT, sib_Pos: [rep64: 11 ], sib_PosOffsetInfo: OMIT} } Attach:[6] Enter Test Step ts_ChangeSB1_ValueTag( )
| Attach:[6] Exit Test Step ts_ChangeSB1_ValueTag
Attach:[7] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:13.460 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[7] Exit Test Step ts_Scheduling
00:00:13.470 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[8] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} Attach:[9] Enter Test Step ts_SendSIB12_LongNeighCellInfo::lt_CompleteSIB( systemInformationBlockType12 )
| 00:00:13.470 - Primitive: RLC_TR_DATA_REQ 00:00:13.470 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[73] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[9] Exit Test Step ts_SendSIB12_LongNeighCellInfo::lt_CompleteSIB
Attach:[10] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:13.470 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[10] Exit Test Step ts_Scheduling
00:00:13.490 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[11] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} 00:00:13.490 - Primitive: RLC_TR_DATA_REQ 00:00:13.490 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[12] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[13] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:13.490 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[13] Exit Test Step ts_Scheduling
00:00:13.500 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[14] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} 00:00:13.500 - Primitive: RLC_TR_DATA_REQ 00:00:13.500 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[15] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[16] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:13.500 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[16] Exit Test Step ts_Scheduling
00:00:13.520 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[17] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} Attach:[18] Enter Test Step ts_SendSIB12_LongNeighCellInfo::lt_CompleteSIB7( { fach_MeasurementOcca ...
| (view Test Step parameters) Assignment:[74] tcv_Segs := (view Assignment) 00:00:13.520 - Primitive: RLC_TR_DATA_REQ 00:00:13.520 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[80] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[18] Exit Test Step ts_SendSIB12_LongNeighCellInfo::lt_CompleteSIB7
Attach:[15] Exit Test Step ts_SendSIB12_LongNeighCellInfo
Attach:[16] Enter Test Step ts_SendSIB18_LongNeighCellInfo( { idleModePLMNIdentiti ...
| (view Test Step parameters) Assignment:[1] tcv_SIB18 := (view Assignment) Assignment:[1] seg1 := '100000'B Assignment:[1] seg2 := '100000101000000010000001'B Attach:[4] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:13.520 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[4] Exit Test Step ts_Scheduling
00:00:13.540 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[5] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} 00:00:13.540 - Primitive: RLC_TR_DATA_REQ 00:00:13.540 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[6] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Assignment:[7] sysInfoType18 := 2 Attach:[8] Enter Test Step ts_ChangeSB1_ValueTag( )
| Attach:[8] Exit Test Step ts_ChangeSB1_ValueTag
Attach:[16] Exit Test Step ts_SendSIB18_LongNeighCellInfo
Attach:[17] Enter Test Step ts_SendSB1_LongNeighCellInfo( { sib_ReferenceList: [ ...
| (view Test Step parameters) Assignment:[1] tcv_Segs := (view Assignment) Attach:[3] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:13.540 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[3] Exit Test Step ts_Scheduling
00:00:13.550 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[4] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} Attach:[5] Enter Test Step ts_SendSB1_LongNeighCellInfo::lt_CompleteSIB( schedulingBlock1 )
| 00:00:13.550 - Primitive: RLC_TR_DATA_REQ 00:00:13.550 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[12] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[5] Exit Test Step ts_SendSB1_LongNeighCellInfo::lt_CompleteSIB
Attach:[6] Enter Test Step ts_ChangeSB1_ValueTag( )
| Attach:[6] Exit Test Step ts_ChangeSB1_ValueTag
Assignment:[7] scheduling := { scheduling: { segCount: OMIT, sib_Pos: [rep16: 1 ], sib_PosOffsetInfo: OMIT} } Assignment:[7] tcv_SB1_ValueTagChanged := GcFALSE Attach:[17] Exit Test Step ts_SendSB1_LongNeighCellInfo
Attach:[18] Enter Test Step ts_SendMIB( { mib_ValueTag: 1 , pl ...
| (view Test Step parameters) Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Assignment:[2] mcc := [ 0 , 0 , 1 ] Assignment:[2] mnc := [ 0 , 1 ] Assignment:[3] tcv_Segs := (view Assignment) Attach:[6] Enter Test Step ts_Scheduling( 0 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:13.550 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[6] Exit Test Step ts_Scheduling
00:00:13.570 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[7] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} Attach:[8] Enter Test Step ts_SendMIB::lt_CompleteSIB( masterInformationBlock )
| 00:00:13.570 - Primitive: RLC_TR_DATA_REQ 00:00:13.570 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[13] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[8] Exit Test Step ts_SendMIB::lt_CompleteSIB
Assignment:[9] tcv_MIB_ValueTagChanged := GcFALSE Attach:[18] Exit Test Step ts_SendMIB
Attach:[3] Exit Test Step ts_SendDefSysInfo_LongNeighCellInfo
Attach:[4] Enter Test Step ts_SaveBackMIB_SB1( 0 )
| Assignment:[2] tcv_MIB_CellA := (view Assignment) Assignment:[2] tcv_SB1_CellA := (view Assignment) Attach:[4] Exit Test Step ts_SaveBackMIB_SB1
Attach:[5] Exit Test Step ts_SendDef_sysInfo_MultiCell
Attach:[6] Enter Test Step ts_SS_CreateCellFACH( 3 )
| Attach:[1] Enter Test Step ts_SS_CellCfg( 3 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 3 )
| Assignment:[8] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[4] Enter Test Step ts_SS_CellCfg::lt_CelllsAlreadyStarted( 3 )
| Attach:[11] Enter Test Step ts_CountConfiguredCell( )
| Assignment:[1] tcv_NumCfgCell := 0 Attach:[2] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 0 , frequenc ...
| (view Test Step parameters) Assignment:[11] tcv_NumCfgCell := 1 Attach:[2] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[3] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 1 , frequenc ...
| (view Test Step parameters) Attach:[3] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[4] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 2 , frequenc ...
| (view Test Step parameters) Attach:[4] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[5] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 3 , frequenc ...
| (view Test Step parameters) Attach:[5] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[6] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 4 , frequenc ...
| (view Test Step parameters) Attach:[6] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[7] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 5 , frequenc ...
| (view Test Step parameters) Attach:[7] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[8] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 6 , frequenc ...
| (view Test Step parameters) Attach:[8] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[9] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 7 , frequenc ...
| (view Test Step parameters) Attach:[9] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[11] Exit Test Step ts_CountConfiguredCell
Attach:[4] Exit Test Step ts_SS_CellCfg::lt_CelllsAlreadyStarted
00:00:13.570 - Primitive: CPHY_Cell_Config_REQ Send event:[6] CPHY ! CPHY_Cell_Config_REQ = PDU (view PDU) 00:00:13.680 - Primitive: CPHY_Cell_Config_CNF begin "ca_CellCfgCnf" of type CPHY_Cell_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER end "ca_CellCfgCnf" of type CPHY_Cell_Config_CNF Receive event:[7] CPHY ? CPHY_Cell_Config_CNF = PDU: { cellId: 3 } Attach:[8] Enter Test Step ts_SaveCellInfo( 3 )
| Assignment:[8] tcv_CellInfoD := (view Assignment) Attach:[8] Exit Test Step ts_SaveCellInfo
Attach:[1] Exit Test Step ts_SS_CellCfg
Attach:[2] Enter Test Step ts_SS_BCH_SCH_CPICH_Cfg( 3 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 3 )
| Assignment:[8] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
00:00:13.680 - Primitive: CPHY_RL_Setup_REQ Send event:[3] CPHY ! CPHY_RL_Setup_REQ = PDU (view PDU) 00:00:13.850 - Primitive: CPHY_RL_Setup_CNF begin "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF Receive event:[4] CPHY ? CPHY_RL_Setup_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 0 ]} 00:00:13.850 - Primitive: CPHY_RL_Setup_REQ Send event:[5] CPHY ! CPHY_RL_Setup_REQ = PDU (view PDU) 00:00:13.880 - Primitive: CPHY_RL_Setup_CNF begin "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF Receive event:[6] CPHY ? CPHY_RL_Setup_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 1 ]} 00:00:13.880 - Primitive: CPHY_RL_Setup_REQ Send event:[7] CPHY ! CPHY_RL_Setup_REQ = PDU (view PDU) 00:00:14.020 - Primitive: CPHY_RL_Setup_CNF begin "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF Receive event:[8] CPHY ? CPHY_RL_Setup_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 2 ]} 00:00:14.020 - Primitive: CPHY_RL_Setup_REQ Send event:[9] CPHY ! CPHY_RL_Setup_REQ = PDU (view PDU) 00:00:14.100 - Primitive: CPHY_RL_Setup_CNF begin "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF Receive event:[10] CPHY ? CPHY_RL_Setup_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 4 ]} 00:00:14.100 - Primitive: CPHY_TrCH_Config_REQ Send event:[11] CPHY ! CPHY_TrCH_Config_REQ = PDU (view PDU) 00:00:14.130 - Primitive: CPHY_TrCH_Config_CNF begin "ca_TrChCfgCnf" of type CPHY_TrCH_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_TrChCfgCnf" of type CPHY_TrCH_Config_CNF Receive event:[12] CPHY ? CPHY_TrCH_Config_CNF = PDU (view PDU) 00:00:14.130 - Primitive: CMAC_Config_REQ Send event:[13] CMAC ! CMAC_Config_REQ = PDU (view PDU) 00:00:14.160 - Primitive: CMAC_Config_CNF begin "ca_CMAC_CfgCnf" of type CMAC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_CfgCnf" of type CMAC_Config_CNF Receive event:[14] CMAC ? CMAC_Config_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 4 ]} Attach:[2] Exit Test Step ts_SS_BCH_SCH_CPICH_Cfg
Attach:[3] Enter Test Step ts_CountConfiguredCell( )
| Assignment:[1] tcv_NumCfgCell := 0 Attach:[2] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 0 , frequenc ...
| (view Test Step parameters) Assignment:[11] tcv_NumCfgCell := 1 Attach:[2] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[3] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 1 , frequenc ...
| (view Test Step parameters) Attach:[3] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[4] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 2 , frequenc ...
| (view Test Step parameters) Attach:[4] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[5] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 3 , frequenc ...
| (view Test Step parameters) Attach:[5] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[6] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 4 , frequenc ...
| (view Test Step parameters) Attach:[6] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[7] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 5 , frequenc ...
| (view Test Step parameters) Attach:[7] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[8] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 6 , frequenc ...
| (view Test Step parameters) Attach:[8] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[9] Enter Test Step ts_CountConfiguredCell::lt_CheckOneCell( { cellId: 7 , frequenc ...
| (view Test Step parameters) Attach:[9] Exit Test Step ts_CountConfiguredCell::lt_CheckOneCell
Attach:[3] Exit Test Step ts_CountConfiguredCell
Attach:[15] Enter Test Step ts_SS_PCH_FACH_CCCH_Cfg( 3 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 3 )
| Assignment:[8] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
00:00:14.160 - Primitive: CPHY_RL_Setup_REQ Send event:[3] CPHY ! CPHY_RL_Setup_REQ = PDU (view PDU) 00:00:14.330 - Primitive: CPHY_RL_Setup_CNF begin "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 5 against 5 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF Receive event:[4] CPHY ? CPHY_RL_Setup_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 5 ]} 00:00:14.330 - Primitive: CPHY_TrCH_Config_REQ Send event:[5] CPHY ! CPHY_TrCH_Config_REQ = PDU (view PDU) 00:00:14.360 - Primitive: CPHY_TrCH_Config_CNF begin "ca_TrChCfgCnf" of type CPHY_TrCH_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 5 against 5 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_TrChCfgCnf" of type CPHY_TrCH_Config_CNF Receive event:[6] CPHY ? CPHY_TrCH_Config_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 5 ]} 00:00:14.360 - Primitive: CMAC_Config_REQ Send event:[7] CMAC ! CMAC_Config_REQ = PDU (view PDU) 00:00:14.380 - Primitive: CMAC_Config_CNF begin "ca_CMAC_CfgCnf" of type CMAC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 5 against 5 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_CfgCnf" of type CMAC_Config_CNF Receive event:[8] CMAC ? CMAC_Config_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 5 ]} 00:00:14.380 - Primitive: CPHY_RL_Setup_REQ Send event:[9] CPHY ! CPHY_RL_Setup_REQ = PDU (view PDU) 00:00:14.490 - Primitive: CPHY_RL_Setup_CNF begin "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF Receive event:[10] CPHY ? CPHY_RL_Setup_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 6 ]} Attach:[15] Exit Test Step ts_SS_PCH_FACH_CCCH_Cfg
Attach:[16] Enter Test Step ts_SS_RACH_CCCH_Cfg( 3 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 3 )
| Assignment:[8] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
00:00:14.490 - Primitive: CPHY_RL_Setup_REQ Send event:[3] CPHY ! CPHY_RL_Setup_REQ = PDU (view PDU) 00:00:14.540 - Primitive: CPHY_RL_Setup_CNF begin "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 7 against 7 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF Receive event:[4] CPHY ? CPHY_RL_Setup_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 7 ]} 00:00:14.540 - Primitive: CPHY_RL_Setup_REQ Send event:[5] CPHY ! CPHY_RL_Setup_REQ = PDU (view PDU) 00:00:14.550 - Primitive: CPHY_RL_Setup_CNF begin "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 8 against 8 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF Receive event:[6] CPHY ? CPHY_RL_Setup_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 8 ]} 00:00:14.550 - Primitive: CPHY_TrCH_Config_REQ Send event:[7] CPHY ! CPHY_TrCH_Config_REQ = PDU (view PDU) 00:00:14.720 - Primitive: CPHY_TrCH_Config_CNF begin "ca_TrChCfgCnf" of type CPHY_TrCH_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 8 against 8 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_TrChCfgCnf" of type CPHY_TrCH_Config_CNF Receive event:[8] CPHY ? CPHY_TrCH_Config_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 8 ]} 00:00:14.720 - Primitive: CMAC_Config_REQ Send event:[9] CMAC ! CMAC_Config_REQ = PDU (view PDU) 00:00:14.750 - Primitive: CMAC_Config_CNF begin "ca_CMAC_CfgCnf" of type CMAC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 8 against 8 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_CfgCnf" of type CMAC_Config_CNF Receive event:[10] CMAC ? CMAC_Config_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 8 ]} Attach:[16] Exit Test Step ts_SS_RACH_CCCH_Cfg
Attach:[17] Enter Test Step ts_SS_RB_BCCH_BCH_Cfg( 3 )
| 00:00:14.750 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:00:14.800 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} Attach:[17] Exit Test Step ts_SS_RB_BCCH_BCH_Cfg
Attach:[18] Enter Test Step ts_SS_RB_PCCH_Cfg( 3 )
| 00:00:14.800 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:00:14.970 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -2 against -2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -2 ]} Attach:[18] Exit Test Step ts_SS_RB_PCCH_Cfg
Attach:[19] Enter Test Step ts_SS_RB0_Cfg( 3 )
| 00:00:14.970 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:00:15.140 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: 0 ]} 00:00:15.140 - Primitive: CRLC_Config_REQ Send event:[3] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:00:15.180 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[4] CRLC ? CRLC_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: 0 ]} Attach:[19] Exit Test Step ts_SS_RB0_Cfg
Attach:[20] Enter Test Step ts_SetCellCfg( 3 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 3 )
| Assignment:[8] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Assignment:[2] cellConfig := cell_FACH_NoDedicated Attach:[3] Enter Test Step ts_SaveCellInfo( 3 )
| Assignment:[8] tcv_CellInfoD := (view Assignment) Attach:[3] Exit Test Step ts_SaveCellInfo
Attach:[20] Exit Test Step ts_SetCellCfg
Attach:[6] Exit Test Step ts_SS_CreateCellFACH
Attach:[7] Enter Test Step ts_SendDef_sysInfo_MultiCell( 3 )
| Attach:[1] Enter Test Step ts_InitializeSIB11_SIB12( 3 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 3 )
| Assignment:[8] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[3] Enter Test Step ts_InitializeSIB11_SIB12::lt_1Or2PLMN( 3 )
| Assignment:[16] tcv_SIB11 := (view Assignment) Assignment:[16] tcv_SIB12 := (view Assignment) Attach:[3] Exit Test Step ts_InitializeSIB11_SIB12::lt_1Or2PLMN
Attach:[1] Exit Test Step ts_InitializeSIB11_SIB12
Attach:[2] Enter Test Step ts_InitMIB_SB1( 3 )
| Assignment:[8] tcv_MIB := (view Assignment) Assignment:[8] tcv_SB1 := (view Assignment) Attach:[2] Exit Test Step ts_InitMIB_SB1
Attach:[3] Enter Test Step ts_SendDefSysInfo_LongNeighCellInfo( 3 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 3 )
| Assignment:[8] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[2] Enter Test Step ts_UTRAN_GERAN_ParaInit( 3 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 3 )
| Assignment:[8] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Assignment:[3] tcv_SIB3 := (view Assignment) Assignment:[3] tcv_SIB4 := (view Assignment) Attach:[2] Exit Test Step ts_UTRAN_GERAN_ParaInit
Attach:[3] Enter Test Step ts_CellDependentPara( 3 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 3 )
| Assignment:[8] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Assignment:[9] cellIdentity := '0000000000000000000000000011'B Assignment:[9] cellIdentity := '0000000000000000000000000011'B Attach:[3] Exit Test Step ts_CellDependentPara
Attach:[4] Enter Test Step ts_InitializeSIB2AndSIB18( { cellId: 3 , frequenc ...
| (view Test Step parameters) Assignment:[1] tcv_SIB2 := { ura_IdentityList: [ '0000000000000010'B ] , nonCriticalExtensions: OMIT} Assignment:[3] tcv_SIB18 := (view Assignment) Attach:[4] Exit Test Step ts_InitializeSIB2AndSIB18
Assignment:[5] tcv_MIB := (view Assignment) Assignment:[5] tcv_SB1 := (view Assignment) Attach:[7] Enter Test Step ts_SendSIB1_LongNeighCellInfo( { cn_CommonGSM_MAP_NAS ...
| (view Test Step parameters) Assignment:[1] tcv_SIB1 := (view Assignment) Assignment:[1] seg1 := (view Assignment) Assignment:[1] seg2 := '00000000000000000010'B Attach:[4] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:15.210 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[4] Exit Test Step ts_Scheduling
00:00:15.220 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[5] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} 00:00:15.220 - Primitive: RLC_TR_DATA_REQ 00:00:15.220 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[6] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Assignment:[7] sysInfoType1 := 2 Attach:[8] Enter Test Step ts_ChangeMIB_ValueTag( )
| Assignment:[2] mib_ValueTag := 2 Assignment:[2] tcv_MIB_ValueTagChanged := GcTRUE Attach:[8] Exit Test Step ts_ChangeMIB_ValueTag
Attach:[7] Exit Test Step ts_SendSIB1_LongNeighCellInfo
Attach:[8] Enter Test Step ts_SendSIB2_LongNeighCellInfo( { ura_IdentityList: [ ...
| (view Test Step parameters) Assignment:[1] tcv_SIB2 := { ura_IdentityList: [ '0000000000000010'B ] , nonCriticalExtensions: OMIT} Assignment:[1] seg1 := '00000000000000000010'B Assignment:[1] seg2 := (view Assignment) Attach:[4] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:15.220 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[4] Exit Test Step ts_Scheduling
00:00:15.240 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[5] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} 00:00:15.240 - Primitive: RLC_TR_DATA_REQ 00:00:15.240 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[6] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Assignment:[7] sysInfoType2 := 2 Attach:[8] Enter Test Step ts_ChangeMIB_ValueTag( )
| Attach:[8] Exit Test Step ts_ChangeMIB_ValueTag
Attach:[8] Exit Test Step ts_SendSIB2_LongNeighCellInfo
Attach:[9] Enter Test Step ts_SendSIB3_LongNeighCellInfo( { sib4indicator: GcTRU ...
| (view Test Step parameters) Assignment:[1] tcv_SIB3 := (view Assignment) Assignment:[1] seg1 := (view Assignment) Assignment:[1] seg2 := '100000101000000010000001'B Attach:[4] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:15.240 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[4] Exit Test Step ts_Scheduling
00:00:15.250 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[5] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} 00:00:15.250 - Primitive: RLC_TR_DATA_REQ 00:00:15.250 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[6] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Assignment:[7] sysInfoType3 := 2 Attach:[8] Enter Test Step ts_ChangeMIB_ValueTag( )
| Attach:[8] Exit Test Step ts_ChangeMIB_ValueTag
Attach:[9] Exit Test Step ts_SendSIB3_LongNeighCellInfo
Attach:[10] Enter Test Step ts_SendSIB4_LongNeighCellInfo( { cellIdentity: '00000 ...
| (view Test Step parameters) Assignment:[1] tcv_SIB4 := (view Assignment) Assignment:[1] seg1 := (view Assignment) Assignment:[1] seg2 := '100000101000000010000001'B Attach:[4] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:15.250 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[4] Exit Test Step ts_Scheduling
00:00:15.270 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[5] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} 00:00:15.270 - Primitive: RLC_TR_DATA_REQ 00:00:15.270 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[6] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Assignment:[7] sysInfoType4 := 2 Attach:[8] Enter Test Step ts_ChangeMIB_ValueTag( )
| Attach:[8] Exit Test Step ts_ChangeMIB_ValueTag
Attach:[10] Exit Test Step ts_SendSIB4_LongNeighCellInfo
Attach:[11] Enter Test Step ts_SendSIB5_LongNeighCellInfo( { sib6indicator: GcTRU ...
| (view Test Step parameters) Assignment:[1] tcv_Segs := (view Assignment) Assignment:[38] sysInfoType5 := 2 Assignment:[38] scheduling := (view Assignment) Attach:[39] Enter Test Step ts_ChangeMIB_ValueTag( )
| Attach:[39] Exit Test Step ts_ChangeMIB_ValueTag
Attach:[40] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:15.300 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[40] Exit Test Step ts_Scheduling
00:00:15.320 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[41] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} 00:00:15.320 - Primitive: RLC_TR_DATA_REQ 00:00:15.320 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[42] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[43] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:15.320 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[43] Exit Test Step ts_Scheduling
00:00:15.330 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[44] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} 00:00:15.330 - Primitive: RLC_TR_DATA_REQ 00:00:15.330 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[45] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[46] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:15.330 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[46] Exit Test Step ts_Scheduling
00:00:15.350 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[47] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} 00:00:15.350 - Primitive: RLC_TR_DATA_REQ 00:00:15.350 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[48] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[49] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:15.350 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[49] Exit Test Step ts_Scheduling
00:00:15.360 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[50] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} 00:00:15.360 - Primitive: RLC_TR_DATA_REQ 00:00:15.360 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[52] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[11] Exit Test Step ts_SendSIB5_LongNeighCellInfo
Attach:[12] Enter Test Step ts_SendSIB6_LongNeighCellInfo( { pich_PowerOffset: -5 ...
| (view Test Step parameters) Assignment:[1] tcv_Segs := (view Assignment) Assignment:[5] sysInfoType6 := 2 Assignment:[5] scheduling := { scheduling: { segCount: OMIT, sib_Pos: [rep64: 2 ], sib_PosOffsetInfo: OMIT} } Attach:[6] Enter Test Step ts_ChangeSB1_ValueTag( )
| Assignment:[2] tcv_SB1_ValueTag := 2 Assignment:[2] sysInfoTypeSB1 := 2 Assignment:[2] tcv_SB1_ValueTagChanged := GcTRUE Attach:[3] Enter Test Step ts_ChangeMIB_ValueTag( )
| Attach:[3] Exit Test Step ts_ChangeMIB_ValueTag
Attach:[6] Exit Test Step ts_ChangeSB1_ValueTag
Attach:[7] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:15.360 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[7] Exit Test Step ts_Scheduling
00:00:15.380 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[8] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} Attach:[9] Enter Test Step ts_SendSIB6_LongNeighCellInfo::lt_CompleteSIB( systemInformationBlockType6 )
| 00:00:15.380 - Primitive: RLC_TR_DATA_REQ 00:00:15.380 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[76] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[9] Exit Test Step ts_SendSIB6_LongNeighCellInfo::lt_CompleteSIB
Attach:[10] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:15.380 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[10] Exit Test Step ts_Scheduling
00:00:15.390 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[11] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} 00:00:15.390 - Primitive: RLC_TR_DATA_REQ 00:00:15.390 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[12] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[13] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:15.390 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[13] Exit Test Step ts_Scheduling
00:00:15.410 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[14] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} 00:00:15.410 - Primitive: RLC_TR_DATA_REQ 00:00:15.410 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[15] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[16] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:15.410 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[16] Exit Test Step ts_Scheduling
00:00:15.430 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[17] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} 00:00:15.430 - Primitive: RLC_TR_DATA_REQ 00:00:15.430 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[18] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[12] Exit Test Step ts_SendSIB6_LongNeighCellInfo
Attach:[13] Enter Test Step ts_SendSIB7_LongNeighCellInfo( { modeSpecificInfo: [f ...
| (view Test Step parameters) Assignment:[1] tcv_Segs := (view Assignment) Assignment:[1] tcv_SIB7 := (view Assignment) Assignment:[1] tcv_Segs_SIB12 := (view Assignment) Attach:[4] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:15.430 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[4] Exit Test Step ts_Scheduling
00:00:15.440 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[5] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} Attach:[6] Enter Test Step ts_SendSIB7_LongNeighCellInfo::lt_CompleteSIB7OrLastSIB12_CompleteSIB7( { modeSpecificInfo: [f ...
| (view Test Step parameters) 00:00:15.440 - Primitive: RLC_TR_DATA_REQ 00:00:15.440 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[36] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[6] Exit Test Step ts_SendSIB7_LongNeighCellInfo::lt_CompleteSIB7OrLastSIB12_CompleteSIB7
Attach:[7] Enter Test Step ts_SendSIB7_LongNeighCellInfo::lt_ConcatWithSIB3( { modeSpecificInfo: [f ...
| (view Test Step parameters) Assignment:[10] seg2 := (view Assignment) Attach:[13] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:15.440 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[13] Exit Test Step ts_Scheduling
00:00:15.460 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[14] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} 00:00:15.460 - Primitive: RLC_TR_DATA_REQ 00:00:15.460 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[15] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[7] Exit Test Step ts_SendSIB7_LongNeighCellInfo::lt_ConcatWithSIB3
Attach:[8] Enter Test Step ts_SendSIB7_LongNeighCellInfo::lt_ConcatWithSIB18( { modeSpecificInfo: [f ...
| (view Test Step parameters) Assignment:[16] seg2 := '100000'B Attach:[19] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:15.460 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[19] Exit Test Step ts_Scheduling
00:00:15.470 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[20] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} 00:00:15.470 - Primitive: RLC_TR_DATA_REQ 00:00:15.470 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[21] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[8] Exit Test Step ts_SendSIB7_LongNeighCellInfo::lt_ConcatWithSIB18
Attach:[9] Enter Test Step ts_SendSIB7_LongNeighCellInfo::lt_ConcatWithSIB4( { modeSpecificInfo: [f ...
| (view Test Step parameters) Assignment:[22] seg2 := (view Assignment) Attach:[25] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:15.470 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[25] Exit Test Step ts_Scheduling
00:00:15.490 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[26] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} 00:00:15.490 - Primitive: RLC_TR_DATA_REQ 00:00:15.490 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[27] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[9] Exit Test Step ts_SendSIB7_LongNeighCellInfo::lt_ConcatWithSIB4
Attach:[13] Exit Test Step ts_SendSIB7_LongNeighCellInfo
Attach:[14] Enter Test Step ts_SendSIB11_LongNeighCellInfo( { sib12indicator: GcTR ...
| (view Test Step parameters) Assignment:[1] tcv_Segs := (view Assignment) Assignment:[20] sysInfoType11 := 2 Assignment:[20] scheduling := (view Assignment) Attach:[21] Enter Test Step ts_ChangeSB1_ValueTag( )
| Attach:[21] Exit Test Step ts_ChangeSB1_ValueTag
Attach:[22] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:15.500 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[22] Exit Test Step ts_Scheduling
00:00:15.520 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[23] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} 00:00:15.520 - Primitive: RLC_TR_DATA_REQ 00:00:15.520 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[24] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[25] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:15.520 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[25] Exit Test Step ts_Scheduling
00:00:15.540 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[26] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} 00:00:15.540 - Primitive: RLC_TR_DATA_REQ 00:00:15.540 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[27] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[28] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:15.540 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[28] Exit Test Step ts_Scheduling
00:00:15.550 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[29] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} 00:00:15.550 - Primitive: RLC_TR_DATA_REQ 00:00:15.550 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[30] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[31] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:15.550 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[31] Exit Test Step ts_Scheduling
00:00:15.570 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[32] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} 00:00:15.570 - Primitive: RLC_TR_DATA_REQ 00:00:15.570 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[34] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[14] Exit Test Step ts_SendSIB11_LongNeighCellInfo
Attach:[15] Enter Test Step ts_SendSIB12_LongNeighCellInfo( { fach_MeasurementOcca ...
| (view Test Step parameters) Assignment:[1] tcv_Segs_SIB12 := (view Assignment) Assignment:[5] sysInfoType12 := 2 Assignment:[5] scheduling := { scheduling: { segCount: OMIT, sib_Pos: [rep64: 11 ], sib_PosOffsetInfo: OMIT} } Attach:[6] Enter Test Step ts_ChangeSB1_ValueTag( )
| Attach:[6] Exit Test Step ts_ChangeSB1_ValueTag
Attach:[7] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:15.570 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[7] Exit Test Step ts_Scheduling
00:00:15.580 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[8] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} Attach:[9] Enter Test Step ts_SendSIB12_LongNeighCellInfo::lt_CompleteSIB( systemInformationBlockType12 )
| 00:00:15.580 - Primitive: RLC_TR_DATA_REQ 00:00:15.580 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[73] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[9] Exit Test Step ts_SendSIB12_LongNeighCellInfo::lt_CompleteSIB
Attach:[10] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:15.580 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[10] Exit Test Step ts_Scheduling
00:00:15.600 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[11] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} 00:00:15.600 - Primitive: RLC_TR_DATA_REQ 00:00:15.600 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[12] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[13] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:15.600 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[13] Exit Test Step ts_Scheduling
00:00:15.610 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[14] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} 00:00:15.610 - Primitive: RLC_TR_DATA_REQ 00:00:15.610 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[15] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[16] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:15.610 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[16] Exit Test Step ts_Scheduling
00:00:15.630 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[17] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} Attach:[18] Enter Test Step ts_SendSIB12_LongNeighCellInfo::lt_CompleteSIB7( { fach_MeasurementOcca ...
| (view Test Step parameters) Assignment:[74] tcv_Segs := (view Assignment) 00:00:15.630 - Primitive: RLC_TR_DATA_REQ 00:00:15.630 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[80] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[18] Exit Test Step ts_SendSIB12_LongNeighCellInfo::lt_CompleteSIB7
Attach:[15] Exit Test Step ts_SendSIB12_LongNeighCellInfo
Attach:[16] Enter Test Step ts_SendSIB18_LongNeighCellInfo( { idleModePLMNIdentiti ...
| (view Test Step parameters) Assignment:[1] tcv_SIB18 := (view Assignment) Assignment:[1] seg1 := '100000'B Assignment:[1] seg2 := '100000101000000010000001'B Attach:[4] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:15.630 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[4] Exit Test Step ts_Scheduling
00:00:15.640 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[5] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} 00:00:15.640 - Primitive: RLC_TR_DATA_REQ 00:00:15.640 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[6] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Assignment:[7] sysInfoType18 := 2 Attach:[8] Enter Test Step ts_ChangeSB1_ValueTag( )
| Attach:[8] Exit Test Step ts_ChangeSB1_ValueTag
Attach:[16] Exit Test Step ts_SendSIB18_LongNeighCellInfo
Attach:[17] Enter Test Step ts_SendSB1_LongNeighCellInfo( { sib_ReferenceList: [ ...
| (view Test Step parameters) Assignment:[1] tcv_Segs := (view Assignment) Attach:[3] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:15.640 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[3] Exit Test Step ts_Scheduling
00:00:15.660 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[4] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} Attach:[5] Enter Test Step ts_SendSB1_LongNeighCellInfo::lt_CompleteSIB( schedulingBlock1 )
| 00:00:15.660 - Primitive: RLC_TR_DATA_REQ 00:00:15.660 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[12] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[5] Exit Test Step ts_SendSB1_LongNeighCellInfo::lt_CompleteSIB
Attach:[6] Enter Test Step ts_ChangeSB1_ValueTag( )
| Attach:[6] Exit Test Step ts_ChangeSB1_ValueTag
Assignment:[7] scheduling := { scheduling: { segCount: OMIT, sib_Pos: [rep16: 1 ], sib_PosOffsetInfo: OMIT} } Assignment:[7] tcv_SB1_ValueTagChanged := GcFALSE Attach:[17] Exit Test Step ts_SendSB1_LongNeighCellInfo
Attach:[18] Enter Test Step ts_SendMIB( { mib_ValueTag: 2 , pl ...
| (view Test Step parameters) Attach:[1] Enter Test Step ts_SetTmpCellInfo( 3 )
| Assignment:[8] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Assignment:[2] mcc := [ 0 , 0 , 1 ] Assignment:[2] mnc := [ 0 , 1 ] Assignment:[3] tcv_Segs := (view Assignment) Attach:[6] Enter Test Step ts_Scheduling( 3 )
| Assignment:[1] tcv_BCCH_ModifyTime := 512 00:00:15.660 - Primitive: CMAC_SYSINFO_Config_REQ Send event:[3] CMAC ! CMAC_SYSINFO_Config_REQ = PDU (view PDU) Attach:[6] Exit Test Step ts_Scheduling
00:00:15.680 - Primitive: CMAC_SYSINFO_Config_CNF begin "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_SysInfoCfgCnf" of type CMAC_SYSINFO_Config_CNF Receive event:[7] CMAC ? CMAC_SYSINFO_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} Attach:[8] Enter Test Step ts_SendMIB::lt_CompleteSIB( masterInformationBlock )
| 00:00:15.680 - Primitive: RLC_TR_DATA_REQ 00:00:15.680 - Primitive: RLC_TR_DATA_REQ: SystemInformation-BCH Send event:[13] TM ! RLC_TR_DATA_REQ = PDU (view PDU) Attach:[8] Exit Test Step ts_SendMIB::lt_CompleteSIB
Assignment:[9] tcv_MIB_ValueTagChanged := GcFALSE Attach:[18] Exit Test Step ts_SendMIB
Attach:[3] Exit Test Step ts_SendDefSysInfo_LongNeighCellInfo
Attach:[4] Enter Test Step ts_SaveBackMIB_SB1( 3 )
| Assignment:[8] tcv_MIB_CellD := (view Assignment) Assignment:[8] tcv_SB1_CellD := (view Assignment) Attach:[4] Exit Test Step ts_SaveBackMIB_SB1
Attach:[7] Exit Test Step ts_SendDef_sysInfo_MultiCell
Attach:[8] Enter Test Step ts_IdleUpdated( 0 )
| Attach:[2] Enter Test Step ts_GMM_IdleUpdated( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[3] Enter Test Step ts_GMM_IdleUpdated::lt_IdleUpdated_NMO_I( 0 )
| Attach:[12] Enter Test Step ts_MMI_UE_SwitchOn( )
| 00:00:15.680 - Primitive: MMI_CmdReq Send event:[1] Ut ! MMI_CmdReq = PDU: { cmd: "Please switch on the UE" } 00:00:20.440 - Primitive: MMI_CmdCnf begin "ca_MMI_CmdCnf" of type MMI_CmdCnf (SEQUENCE) [UNIVERSAL 16] begin "result" of type BOOLEAN [UNIVERSAL 1] matching GcTRUE against GcTRUE end "result" of type BOOLEAN end "ca_MMI_CmdCnf" of type MMI_CmdCnf Receive event:[2] Ut ? MMI_CmdCnf = PDU: { result: GcTRUE , resultString: OMIT} Attach:[12] Exit Test Step ts_MMI_UE_SwitchOn
Attach:[13] Enter Test Step ts_RRC_ConnEst( 0 )
| Attach:[1] Enter Test Step ts_SS_PrepareCellRRC_ConnEst( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[1] Exit Test Step ts_SS_PrepareCellRRC_ConnEst
Attach:[2] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[2] Exit Test Step ts_SetTmpCellInfo
Attach:[3] Enter Test Step ts_RRC_ConnEst::lt_RcvConnReq( 0 )
| 00:00:30.830 - Primitive: RLC_TR_DATA_IND: rrcConnectionRequest 00:00:30.830 - Primitive: RLC_TR_DATA_IND begin "car_RRC_ConnReq" of type RLC_TR_DATA_IND (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "tM_message" of type CHOICE [UNIVERSAL 31] begin "uL_CCCH_Message" of type UL_CCCH_Message (SEQUENCE) [UNIVERSAL 16] begin "message" of type UL_CCCH_MessageType (CHOICE) [UNIVERSAL 31] begin "rrcConnectionRequest" of type RRCConnectionRequest (SEQUENCE) [UNIVERSAL 16] begin "initialUE_Identity" of type InitialUE_Identity (CHOICE) [UNIVERSAL 31] begin InitialUE_Identity (CHOICE) [UNIVERSAL 31] end InitialUE_Identity begin InitialUE_Identity (CHOICE) [UNIVERSAL 31] begin "tmsi_and_LAI" of type TMSI_and_LAI_GSM_MAP (SEQUENCE) [UNIVERSAL 16] matching { tmsi: '00010001001000100011001101000100'B , lai: { plmn_Identity: { mcc: [ 0 , 0 , 1 ] , mnc: [ 0 , 1 ] } , lac: '0000000000000001'B } } against ? end "tmsi_and_LAI" of type TMSI_and_LAI_GSM_MAP end InitialUE_Identity matching [tmsi_and_LAI: { tmsi: '00010001001000100011001101000100'B , lai: { plmn_Identity: { mcc: [ 0 , 0 , 1 ] , mnc: [ 0 , 1 ] } , lac: '0000000000000001'B } } ] against ([imsi: ?], [tmsi_and_LAI: ?], [p_TMSI_and_RAI: ?], [imei: ?]) end "initialUE_Identity" of type InitialUE_Identity begin "establishmentCause" of type EstablishmentCause (ENUMERATED) [UNIVERSAL 10] matching registration against registration end "establishmentCause" of type EstablishmentCause begin "protocolErrorIndicator" of type ProtocolErrorIndicator (ENUMERATED) [UNIVERSAL 10] matching noError against noError end "protocolErrorIndicator" of type ProtocolErrorIndicator end "rrcConnectionRequest" of type RRCConnectionRequest end "message" of type UL_CCCH_MessageType end "uL_CCCH_Message" of type UL_CCCH_Message end "tM_message" of type CHOICE end "car_RRC_ConnReq" of type RLC_TR_DATA_IND Assignment:[7] tcv_InitialUE_Id := (view Assignment) Receive event:[7] TM ? RLC_TR_DATA_IND = PDU (view PDU) Attach:[3] Exit Test Step ts_RRC_ConnEst::lt_RcvConnReq
Attach:[4] Enter Test Step ts_RRC_ConnEst::lt_Send_ConnSetUp( 0 )
| 00:00:30.830 - Primitive: RLC_UM_DATA_REQ 00:00:30.830 - Primitive: RLC_UM_DATA_REQ: rrcConnectionSetup Send event:[31] UM ! RLC_UM_DATA_REQ = PDU (view PDU) Attach:[33] Enter Test Step ts_SetCellCfg( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Assignment:[2] cellConfig := cell_DCH_StandAloneSRB Attach:[3] Enter Test Step ts_SaveCellInfo( 0 )
| Assignment:[2] tcv_CellInfoA := (view Assignment) Attach:[3] Exit Test Step ts_SaveCellInfo
Attach:[33] Exit Test Step ts_SetCellCfg
Attach:[4] Exit Test Step ts_RRC_ConnEst::lt_Send_ConnSetUp
Attach:[5] Enter Test Step ts_RRC_ReceiveConnSetupCmpl( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
StartTimer:[3] t_WaitMS [13500] 13500 ms 00:00:31.460 - Primitive: RLC_AM_DATA_IND: rrcConnectionSetupComplete 00:00:31.470 - Primitive: RLC_AM_DATA_IND begin "car_RRC_ConnSetupCmpl" of type RLC_AM_DATA_IND (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "integrityResult" of type IntegrityResult (CHOICE) [UNIVERSAL 31] matching [integrityUsed: i_pass] against ? end "integrityResult" of type IntegrityResult begin "aM_message" of type CHOICE [UNIVERSAL 31] begin "uL_DCCH_Message" of type UL_DCCH_Message (SEQUENCE) [UNIVERSAL 16] begin "message" of type UL_DCCH_MessageType (CHOICE) [UNIVERSAL 31] begin "rrcConnectionSetupComplete" of type RRCConnectionSetupComplete (SEQUENCE) [UNIVERSAL 16] begin "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier (INTEGER) [UNIVERSAL 2] matching 0 against 0 end "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier begin "startList" of type STARTList (SEQUENCEOF) [UNIVERSAL 28] matching [ { cn_DomainIdentity: ps_domain, start_Value: '00000000000000000010'B } , { cn_DomainIdentity: cs_domain, start_Value: '00000000000000000100'B } ] against ? end "startList" of type STARTList begin "ue_RadioAccessCapability" of type UE_RadioAccessCapability (SEQUENCE) [UNIVERSAL 16] matching { accessStratumReleaseIndicator: r99, pdcp_Capability: { losslessSRNS_RelocationSupport: GcTRUE , supportForRfc2507: [supported: by8192]} , rlc_Capability: { totalRLC_AM_BufferSize: kb50, maximumRLC_WindowSize: mws2047, maximumAM_EntityNumber: am6} , transportChannelCapability: { dl_TransChCapability: { maxNoBitsReceived: b5120, maxConvCodeBitsReceived: b1280, turboDecodingSupport: [supported: b5120], maxSimultaneousTransChs: e8, maxSimultaneousCCTrCH_Count: 1 , maxReceivedTransportBlocks: tb16, maxNumberOfTFC: tfc96, maxNumberOfTF: tf64} , ul_TransChCapability: { maxNoBitsTransmitted: b3840, maxConvCodeBitsTransmitted: b1280, turboEncodingSupport: [supported: b3840], maxSimultaneousTransChs: e8, modeSpecificInfo: [fdd: NULL], maxTransmittedBlocks: tb8, maxNumberOfTFC: tfc32, maxNumberOfTF: tf32} } , rf_Capability: { fddRF_Capability: { ue_PowerClass: 4 , txRxFrequencySeparation: mhz190} , tddRF_Capability: OMIT} , physicalChannelCapability: { fddPhysChCapability: { downlinkPhysChCapability: { maxNoDPCH_PDSCH_Codes: 3 , maxNoPhysChBitsReceived: b9600, supportForSF_512: GcFALSE , supportOfPDSCH: GcFALSE , simultaneousSCCPCH_DPCH_Reception: [notSupported: NULL]} , uplinkPhysChCapability: { maxNoDPDCH_BitsTransmitted: b2400, supportOfPCPCH: GcFALSE } } , tddPhysChCapability: OMIT} , ue_MultiModeRAT_Capability: { multiRAT_CapabilityList: { supportOfGSM: GcFALSE , supportOfMulticarrier: GcFALSE } , multiModeCapability: fdd} , securityCapability: { cipheringAlgorithmCap: '0000000000000001'B , integrityProtectionAlgorithmCap: '0000000000000010'B } , ue_positioning_Capability: { standaloneLocMethodsSupported: GcFALSE , ue_BasedOTDOA_Supported: GcFALSE , networkAssistedGPS_Supported: noNetworkAssistedGPS, supportForUE_GPS_TimingOfCellFrames: GcFALSE , supportForIPDL: GcFALSE } , measurementCapability: { downlinkCompressedMode: { fdd_Measurements: GcTRUE , tdd_Measurements: OMIT, gsm_Measurements: { gsm900: GcTRUE , dcs1800: GcTRUE , gsm1900: GcFALSE } , multiCarrierMeasurements: GcFALSE } , uplinkCompressedMode: { fdd_Measurements: GcTRUE , tdd_Measurements: OMIT, gsm_Measurements: { gsm900: GcTRUE , dcs1800: GcTRUE , gsm1900: GcFALSE } , multiCarrierMeasurements: GcFALSE } } } against * end "ue_RadioAccessCapability" of type UE_RadioAccessCapability end "rrcConnectionSetupComplete" of type RRCConnectionSetupComplete end "message" of type UL_DCCH_MessageType end "uL_DCCH_Message" of type UL_DCCH_Message end "aM_message" of type CHOICE end "car_RRC_ConnSetupCmpl" of type RLC_AM_DATA_IND Assignment:TSP1: [5] tcv_StartList := (view Assignment) Assignment:TSP1: [5] cipheringAlgorithmCapability := '0000000000000001'B CancelTimer:TSP1: [5] t_WaitMS [13500] 13500 ms Receive event:TSP1: [5] AM ? RLC_AM_DATA_IND = PDU (view PDU) Preliminary verdict:TSP1: [5] (PASS) Attach:[6] Enter Test Step ts_RRC_ReceiveConnSetupCmpl::lt_GetHFN( 0 )
| Assignment:[13] tcv_Count := 2 Attach:[17] Enter Test Step ts_RRC_ReceiveConnSetupCmpl::lt_FirstValue( 0 )
| Assignment:[23] start_PS := '00000000000000000010'B Attach:[17] Exit Test Step ts_RRC_ReceiveConnSetupCmpl::lt_FirstValue
Attach:[18] Enter Test Step ts_RRC_ReceiveConnSetupCmpl::lt_SecondValue( 0 )
| Assignment:[26] start_CS := '00000000000000000100'B Attach:[18] Exit Test Step ts_RRC_ReceiveConnSetupCmpl::lt_SecondValue
Attach:[6] Exit Test Step ts_RRC_ReceiveConnSetupCmpl::lt_GetHFN
Attach:[5] Exit Test Step ts_RRC_ReceiveConnSetupCmpl
Attach:[13] Exit Test Step ts_RRC_ConnEst
00:00:31.450 - Primitive: RLC_AM_DATA_IND: initialDirectTransfer 00:00:31.450 - Primitive: RRC_DATA_IND: mm:locationUpdatingRequest begin "car_InitDirectTransfer" of type RRC_DataInd (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "rB_Id" of type SS_RB_Identity (INTEGER) [UNIVERSAL 2] matching 3 against 3 end "rB_Id" of type SS_RB_Identity begin "cN_Domain" of type SS_CN_DomainIdentity (INTEGER) [UNIVERSAL 2] matching 0 against 0 end "cN_Domain" of type SS_CN_DomainIdentity begin "start" of type START_Value (BITSTRING) [UNIVERSAL 3] matching '00000000000000000100'B against ? end "start" of type START_Value begin "msg" of type LOCATIONUPDATINGREQUEST (SEQUENCE) [UNIVERSAL 16] begin "skipIndicator" of type SkipIndicator (BITSTRING) [UNIVERSAL 3] matching '0000'B against '0000'B end "skipIndicator" of type SkipIndicator begin "mMProtocolDiscriminator" of type ProtocolDiscriminator (BITSTRING) [UNIVERSAL 3] matching '0101'B against '0101'B end "mMProtocolDiscriminator" of type ProtocolDiscriminator begin "msgType" of type MsgType (BITSTRING) [UNIVERSAL 3] matching '00001000'B against '??001000'B end "msgType" of type MsgType begin "ciphKeySeqNum" of type CiphKeySeqNum (SEQUENCE) [UNIVERSAL 16] begin "spare1" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against '0'B end "spare1" of type B1 begin "keySeq" of type KeySeq (BITSTRING) [UNIVERSAL 3] matching '001'B against ? end "keySeq" of type KeySeq end "ciphKeySeqNum" of type CiphKeySeqNum begin "locUpdType" of type LocUpdType (SEQUENCE) [UNIVERSAL 16] begin "fOR" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against ? end "fOR" of type B1 begin "spare1" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against '0'B end "spare1" of type B1 begin "lUT" of type B2 (BITSTRING) [UNIVERSAL 3] matching '10'B against ? end "lUT" of type B2 end "locUpdType" of type LocUpdType begin "locAreaId" of type LocAreaId_v (SEQUENCE) [UNIVERSAL 16] begin "plmn" of type OCTETSTRING [UNIVERSAL 4] matching '00F110'O against ? end "plmn" of type OCTETSTRING begin "lac" of type OCTETSTRING [UNIVERSAL 4] matching '0001'O against ? end "lac" of type OCTETSTRING end "locAreaId" of type LocAreaId_v begin "mSClsmk1" of type MS_Clsmk1 (SEQUENCE) [UNIVERSAL 16] begin "spare1" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against '0'B end "spare1" of type B1 begin "revLvl" of type B2 (BITSTRING) [UNIVERSAL 3] matching '10'B against ? end "revLvl" of type B2 begin "eSIND" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against ? end "eSIND" of type B1 begin "a5_1" of type B1 (BITSTRING) [UNIVERSAL 3] matching '1'B against ? end "a5_1" of type B1 begin "rFPwrCap" of type B3 (BITSTRING) [UNIVERSAL 3] matching '111'B against ? end "rFPwrCap" of type B3 end "mSClsmk1" of type MS_Clsmk1 begin "mobileId" of type MS_Identity_lv (SEQUENCE) [UNIVERSAL 16] begin "iel" of type Length (OCTETSTRING) [UNIVERSAL 4] matching '05'O against ? end "iel" of type Length begin "iDigit1" of type B4 (BITSTRING) [UNIVERSAL 3] matching '1111'B against ? end "iDigit1" of type B4 begin "oddEvenInd" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against ? end "oddEvenInd" of type B1 begin "typeOfId" of type B3 (BITSTRING) [UNIVERSAL 3] matching '100'B against ? end "typeOfId" of type B3 begin "otherDigits" of type OCTETSTRING [UNIVERSAL 4] matching '11223344'O against ? end "otherDigits" of type OCTETSTRING end "mobileId" of type MS_Identity_lv begin "mSClsmk2" of type MS_Clsmk2 (SEQUENCE) [UNIVERSAL 16] begin "iei" of type IEI8 (BITSTRING) [UNIVERSAL 3] matching '00110011'B against '00110011'B end "iei" of type IEI8 begin "iel" of type Length (OCTETSTRING) [UNIVERSAL 4] matching '03'O against '03'O end "iel" of type Length begin "spare1_1" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against '0'B end "spare1_1" of type B1 begin "revLvl" of type B2 (BITSTRING) [UNIVERSAL 3] matching '10'B against ? end "revLvl" of type B2 begin "eSIND" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against ? end "eSIND" of type B1 begin "a5_1" of type B1 (BITSTRING) [UNIVERSAL 3] matching '1'B against ? end "a5_1" of type B1 begin "rFPwrCap" of type B3 (BITSTRING) [UNIVERSAL 3] matching '111'B against ? end "rFPwrCap" of type B3 begin "spare1_2" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against '0'B end "spare1_2" of type B1 begin "pSCap" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against ? end "pSCap" of type B1 begin "sSSI" of type B2 (BITSTRING) [UNIVERSAL 3] matching '01'B against ? end "sSSI" of type B2 begin "sMCap" of type B1 (BITSTRING) [UNIVERSAL 3] matching '1'B against ? end "sMCap" of type B1 begin "vBS" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against ? end "vBS" of type B1 begin "vGCS" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against ? end "vGCS" of type B1 begin "fC" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against ? end "fC" of type B1 begin "cM3" of type B1 (BITSTRING) [UNIVERSAL 3] matching '1'B against ? end "cM3" of type B1 begin "spare1_3" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against '0'B end "spare1_3" of type B1 begin "lCSVA" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against ? end "lCSVA" of type B1 begin "uCS2" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against ? end "uCS2" of type B1 begin "soLSA" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against ? end "soLSA" of type B1 begin "cMSP" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against ? end "cMSP" of type B1 begin "a5_3" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against ? end "a5_3" of type B1 begin "a5_2" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against ? end "a5_2" of type B1 end "mSClsmk2" of type MS_Clsmk2 end "msg" of type LOCATIONUPDATINGREQUEST end "car_InitDirectTransfer" of type RRC_DataInd Assignment:[21] tcv_Start := '00000000000000000100'B Receive event:[21] Dc ? RRC_DataInd = PDU (view PDU) Attach:[22] Enter Test Step ts_SS_SecurityDownloadStart( cs_domain )
| Assignment:[2] start_CS := '00000000000000000100'B Attach:[22] Exit Test Step ts_SS_SecurityDownloadStart
Attach:[23] Enter Test Step ts_MM_Authentication( 0 )
| Attach:[1] Enter Test Step ts_MM_AuthenticationInit( )
| Attach:[1] Enter Test Step ts_MM_AuthenticationInit::lt_IncrementCiphKeySeqNum( )
| Assignment:[18] tcv_CS_KeySeq := '000'B Attach:[1] Exit Test Step ts_MM_AuthenticationInit::lt_IncrementCiphKeySeqNum
Attach:[2] Enter Test Step ts_MM_AuthenticationInit::lt_AuthCalcAUTN( )
| Assignment:[19] tcv_AuthXDOUT := (view Assignment) Assignment:[20] tcv_AuthCDOUT := '0000000000000000000000000000000000000000000000000000000000000000'B Assignment:[21] tcv_AuthXDOUT_Half := '0101010101000100011101110110011000010001000000000011001100100010'B Assignment:[22] tcv_AuthAK := '011001100001000100000000001100110010001011011101'B Assignment:[23] tcv_AuthAUTN_1 := '011001100001000100000000001100110010001011011101'B Assignment:[24] tcv_AuthMAC := '0101010101000100011101110110011000010001000000000011001100100010'B Assignment:[25] tcv_AuthAUTN_2 := (view Assignment) Assignment:[26] tcv_AuthAUTN := (view Assignment) Attach:[2] Exit Test Step ts_MM_AuthenticationInit::lt_AuthCalcAUTN
Attach:[3] Enter Test Step ts_MM_AuthenticationInit::lt_AuthCalcUMTS_Others( )
| Assignment:[27] tcv_AuthIK := (view Assignment) Assignment:[28] tcv_AuthCK := (view Assignment) Assignment:[29] tcv_AuthXRES := (view Assignment) Attach:[3] Exit Test Step ts_MM_AuthenticationInit::lt_AuthCalcUMTS_Others
Attach:[4] Enter Test Step ts_MM_AuthenticationInit::lt_AuthCalcKcGSM( )
| Assignment:[30] tcv_AuthCK_1 := '0100010001110111011001100001000100000000001100110010001011011101'B Assignment:[31] tcv_AuthCK_2 := '1100110011111111111011101001100110001000101110111010101001010101'B Assignment:[32] tcv_AuthIK_1 := '0111011101100110000100010000000000110011001000101101110111001100'B Assignment:[33] tcv_AuthIK_2 := '1111111111101110100110011000100010111011101010100101010101000100'B Assignment:[34] tcv_AuthCK_XOR := '1000100010001000100010001000100010001000100010001000100010001000'B Assignment:[35] tcv_AuthIK_XOR := '1000100010001000100010001000100010001000100010001000100010001000'B Assignment:[36] tcv_AuthKcGSM := '0000000000000000000000000000000000000000000000000000000000000000'B Attach:[4] Exit Test Step ts_MM_AuthenticationInit::lt_AuthCalcKcGSM
Attach:[1] Exit Test Step ts_MM_AuthenticationInit
00:00:31.500 - Primitive: RRC_DATA_REQ: mm:authenticationRequest 00:00:31.500 - Primitive: RLC_AM_DATA_REQ:downlinkDirectTransfer Send event:[2] Dc ! RRC_DataReq = PDU (view PDU) 00:00:32.010 - Primitive: RLC_AM_DATA_IND: uplinkDirectTransfer 00:00:32.010 - Primitive: RRC_DATA_IND: mm:authenticationResponse begin "car_UplinkDirectTransfer" of type RRC_DataInd (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "rB_Id" of type SS_RB_Identity (INTEGER) [UNIVERSAL 2] matching 3 against 3 end "rB_Id" of type SS_RB_Identity begin "cN_Domain" of type SS_CN_DomainIdentity (INTEGER) [UNIVERSAL 2] matching 0 against 0 end "cN_Domain" of type SS_CN_DomainIdentity begin "msg" of type AUTHENTICATIONRESPONSE (SEQUENCE) [UNIVERSAL 16] begin "skipIndicator" of type SkipIndicator (BITSTRING) [UNIVERSAL 3] matching '0000'B against '0000'B end "skipIndicator" of type SkipIndicator begin "mMProtocolDiscriminator" of type ProtocolDiscriminator (BITSTRING) [UNIVERSAL 3] matching '0101'B against '0101'B end "mMProtocolDiscriminator" of type ProtocolDiscriminator begin "msgType" of type MsgType (BITSTRING) [UNIVERSAL 3] matching '01010100'B against '??010100'B end "msgType" of type MsgType begin "authRsp" of type AuthRsp (BITSTRING) [UNIVERSAL 3] matching '01010101010001000111011101100110'B against ? end "authRsp" of type AuthRsp begin "authRspExt" of type AuthRspExt (SEQUENCE) [UNIVERSAL 16] begin "iei" of type IEI8 (BITSTRING) [UNIVERSAL 3] matching '00100001'B against '00100001'B end "iei" of type IEI8 begin "iel" of type Length (OCTETSTRING) [UNIVERSAL 4] matching '0C'O against ? end "iel" of type Length begin "rES" of type BITSTRING [UNIVERSAL 3] matching '000100010000000000110011001000101101110111001100111111111110111010011001100010001011101110101010'B against ? end "rES" of type BITSTRING end "authRspExt" of type AuthRspExt end "msg" of type AUTHENTICATIONRESPONSE end "car_UplinkDirectTransfer" of type RRC_DataInd Assignment:[3] tcv_AuthRspPDU (view PDU) Assignment:[3] tcv_AuthRsp := '01010101010001000111011101100110'B Assignment:[3] tcv_AuthRspExt := (view Assignment) Receive event:[3] Dc ? RRC_DataInd = PDU (view PDU) Assignment:[4] tcv_Res := GcTRUE Attach:[23] Exit Test Step ts_MM_Authentication
Attach:[24] Enter Test Step ts_RRC_Security( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[2] Enter Test Step ts_RRC_Security::lt_RRC_InitVariables( 0 )
| Attach:[53] Enter Test Step ts_RRC_Security::lt_InitCipherMode( 0 )
| Assignment:[76] dL_CipherMode := [startRestart: uea0] Assignment:[76] cipheringAlgorithmCapability := '0000000000000001'B Assignment:[78] cs_cipheringStarted := GcTRUE Attach:[53] Exit Test Step ts_RRC_Security::lt_InitCipherMode
Attach:[54] Enter Test Step ts_RRC_Security::lt_InitIntegrity( 0 )
| Assignment:[87] recentSecureDomain := cs_domain Assignment:[92] dL_Integrity := (view Assignment) Assignment:[92] integrityStarted := GcTRUE Assignment:[92] dl_IntegrityCheckInfo := (view Assignment) Assignment:[92] tcv_Int_ModifyFlag := GcFALSE Attach:[54] Exit Test Step ts_RRC_Security::lt_InitIntegrity
Attach:[55] Enter Test Step ts_InitSystemSpecificCap( )
| Assignment:[11] tcv_UE_SystemSpecificCap := 0 Attach:[55] Exit Test Step ts_InitSystemSpecificCap
Attach:[56] Enter Test Step ts_SaveCellInfo( 0 )
| Assignment:[2] tcv_CellInfoA := (view Assignment) Attach:[56] Exit Test Step ts_SaveCellInfo
Assignment:[58] tcv_HFN := '00000000000000000000'B Assignment:[60] start_CS := '00000000000000000000'B Attach:[2] Exit Test Step ts_RRC_Security::lt_RRC_InitVariables
Attach:[3] Enter Test Step ts_SS_DownloadSecurityKey( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[6] Enter Test Step ts_SS_DownloadSecurityKey::lt_DownloadKeyCRLC( '00000000000000000000'B )
| 00:00:32.020 - Primitive: CRLC_SecurityMode_Config_REQ 00:00:32.020 - Primitive: CRLC_SecurityMode_Config_REQ Send event:[21] CRLC ! CRLC_SecurityMode_Config_REQ = PDU (view PDU) 00:00:32.040 - Primitive: CRLC_SecurityMode_Config_CNF begin "ca_CRLC_SecurityModeCfgCnf" of type CRLC_SecurityMode_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER end "ca_CRLC_SecurityModeCfgCnf" of type CRLC_SecurityMode_Config_CNF Receive event:[22] CRLC ? CRLC_SecurityMode_Config_CNF = PDU: { cellId: -1 } Attach:[6] Exit Test Step ts_SS_DownloadSecurityKey::lt_DownloadKeyCRLC
Attach:[3] Exit Test Step ts_SS_DownloadSecurityKey
Attach:[4] Enter Test Step ts_RRC_Security::lt_ActivateSecurity_DL_SS( 0 )
| Attach:[14] Enter Test Step ts_RRC_Security::lt_InitialiseRRC_MSN( 0 )
| Attach:[25] Enter Test Step ts_SetDL_RRC_MessageSN( 0 )
| 00:00:32.040 - Primitive: CRLC_SetRRC_MessageSN_REQ Send event:[1] CRLC ! CRLC_SetRRC_MessageSN_REQ = PDU (view PDU) 00:00:32.050 - Primitive: CRLC_SetRRC_MessageSN_CNF begin "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF Receive event:[2] CRLC ? CRLC_SetRRC_MessageSN_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: 0 ]} 00:00:32.050 - Primitive: CRLC_SetRRC_MessageSN_REQ Send event:[3] CRLC ! CRLC_SetRRC_MessageSN_REQ = PDU (view PDU) 00:00:32.070 - Primitive: CRLC_SetRRC_MessageSN_CNF begin "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF Receive event:[4] CRLC ? CRLC_SetRRC_MessageSN_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 1 ]} 00:00:32.070 - Primitive: CRLC_SetRRC_MessageSN_REQ Send event:[5] CRLC ! CRLC_SetRRC_MessageSN_REQ = PDU (view PDU) 00:00:32.080 - Primitive: CRLC_SetRRC_MessageSN_CNF begin "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF Receive event:[6] CRLC ? CRLC_SetRRC_MessageSN_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 2 ]} 00:00:32.080 - Primitive: CRLC_SetRRC_MessageSN_REQ Send event:[7] CRLC ! CRLC_SetRRC_MessageSN_REQ = PDU (view PDU) 00:00:32.100 - Primitive: CRLC_SetRRC_MessageSN_CNF begin "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF Receive event:[8] CRLC ? CRLC_SetRRC_MessageSN_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 3 ]} 00:00:32.100 - Primitive: CRLC_SetRRC_MessageSN_REQ Send event:[9] CRLC ! CRLC_SetRRC_MessageSN_REQ = PDU (view PDU) 00:00:32.110 - Primitive: CRLC_SetRRC_MessageSN_CNF begin "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF Receive event:[10] CRLC ? CRLC_SetRRC_MessageSN_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 4 ]} Attach:[25] Exit Test Step ts_SetDL_RRC_MessageSN
Attach:[14] Exit Test Step ts_RRC_Security::lt_InitialiseRRC_MSN
Attach:[15] Enter Test Step ts_CRLC_DL_Integrity( { integrityProtectionM ...
| (view Test Step parameters) 00:00:32.110 - Primitive: CRLC_Integrity_Activate_REQ 00:00:32.110 - Primitive: CRLC_Integrity_Activate_REQ Send event:[1] CRLC ! CRLC_Integrity_Activate_REQ = PDU (view PDU) 00:00:32.130 - Primitive: CRLC_Integrity_Activate_CNF begin "ca_CRLC_IntegrityActivateCnf" of type CRLC_Integrity_Activate_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER end "ca_CRLC_IntegrityActivateCnf" of type CRLC_Integrity_Activate_CNF Receive event:[2] CRLC ? CRLC_Integrity_Activate_CNF = PDU: { cellId: -1 } Attach:[15] Exit Test Step ts_CRLC_DL_Integrity
Attach:[17] Enter Test Step ts_CRLC_GetRLC_SeqNumSecurity( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
00:00:32.130 - Primitive: CRLC_SequenceNumber_REQ Send event:[2] CRLC ! CRLC_SequenceNumber_REQ = PDU: { cellId: -1 , routingInfo: [rB_Identity: 1 ]} 00:00:32.160 - Primitive: CRLC_SequenceNumber_CNF begin "car_GetRLC_SeqNum" of type CRLC_SequenceNumber_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "count_C_MSB_UL" of type COUNT_C_MSB (INTEGER) [UNIVERSAL 2] matching 0 against ? end "count_C_MSB_UL" of type COUNT_C_MSB begin "count_C_LSB_UL" of type RLC_SequenceNumber (INTEGER) [UNIVERSAL 2] matching 0 against ? end "count_C_LSB_UL" of type RLC_SequenceNumber begin "count_C_MSB_DL" of type COUNT_C_MSB (INTEGER) [UNIVERSAL 2] matching 0 against ? end "count_C_MSB_DL" of type COUNT_C_MSB begin "count_C_LSB_DL" of type RLC_SequenceNumber (INTEGER) [UNIVERSAL 2] matching 0 against ? end "count_C_LSB_DL" of type RLC_SequenceNumber end "car_GetRLC_SeqNum" of type CRLC_SequenceNumber_CNF Assignment:[3] tcv_RLC_SeqNumDL_RB1 := 0 Receive event:[3] CRLC ? CRLC_SequenceNumber_CNF = PDU (view PDU) 00:00:32.160 - Primitive: CRLC_SequenceNumber_REQ Send event:[4] CRLC ! CRLC_SequenceNumber_REQ = PDU: { cellId: -1 , routingInfo: [rB_Identity: 2 ]} 00:00:32.190 - Primitive: CRLC_SequenceNumber_CNF begin "car_GetRLC_SeqNum" of type CRLC_SequenceNumber_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "count_C_MSB_UL" of type COUNT_C_MSB (INTEGER) [UNIVERSAL 2] matching 0 against ? end "count_C_MSB_UL" of type COUNT_C_MSB begin "count_C_LSB_UL" of type RLC_SequenceNumber (INTEGER) [UNIVERSAL 2] matching 2 against ? end "count_C_LSB_UL" of type RLC_SequenceNumber begin "count_C_MSB_DL" of type COUNT_C_MSB (INTEGER) [UNIVERSAL 2] matching 0 against ? end "count_C_MSB_DL" of type COUNT_C_MSB begin "count_C_LSB_DL" of type RLC_SequenceNumber (INTEGER) [UNIVERSAL 2] matching 0 against ? end "count_C_LSB_DL" of type RLC_SequenceNumber end "car_GetRLC_SeqNum" of type CRLC_SequenceNumber_CNF Assignment:[5] tcv_RLC_SeqNumDL_RB2 := 0 Receive event:[5] CRLC ? CRLC_SequenceNumber_CNF = PDU (view PDU) 00:00:32.190 - Primitive: CRLC_SequenceNumber_REQ Send event:[6] CRLC ! CRLC_SequenceNumber_REQ = PDU: { cellId: -1 , routingInfo: [rB_Identity: 3 ]} 00:00:32.220 - Primitive: CRLC_SequenceNumber_CNF begin "car_GetRLC_SeqNum" of type CRLC_SequenceNumber_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "count_C_MSB_UL" of type COUNT_C_MSB (INTEGER) [UNIVERSAL 2] matching 0 against ? end "count_C_MSB_UL" of type COUNT_C_MSB begin "count_C_LSB_UL" of type RLC_SequenceNumber (INTEGER) [UNIVERSAL 2] matching 4 against ? end "count_C_LSB_UL" of type RLC_SequenceNumber begin "count_C_MSB_DL" of type COUNT_C_MSB (INTEGER) [UNIVERSAL 2] matching 0 against ? end "count_C_MSB_DL" of type COUNT_C_MSB begin "count_C_LSB_DL" of type RLC_SequenceNumber (INTEGER) [UNIVERSAL 2] matching 3 against ? end "count_C_LSB_DL" of type RLC_SequenceNumber end "car_GetRLC_SeqNum" of type CRLC_SequenceNumber_CNF Assignment:[7] tcv_RLC_SeqNumDL_RB3 := 3 Receive event:[7] CRLC ? CRLC_SequenceNumber_CNF = PDU (view PDU) 00:00:32.220 - Primitive: CRLC_SequenceNumber_REQ Send event:[8] CRLC ! CRLC_SequenceNumber_REQ = PDU: { cellId: -1 , routingInfo: [rB_Identity: 4 ]} 00:00:32.250 - Primitive: CRLC_SequenceNumber_CNF begin "car_GetRLC_SeqNum" of type CRLC_SequenceNumber_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "count_C_MSB_UL" of type COUNT_C_MSB (INTEGER) [UNIVERSAL 2] matching 0 against ? end "count_C_MSB_UL" of type COUNT_C_MSB begin "count_C_LSB_UL" of type RLC_SequenceNumber (INTEGER) [UNIVERSAL 2] matching 0 against ? end "count_C_LSB_UL" of type RLC_SequenceNumber begin "count_C_MSB_DL" of type COUNT_C_MSB (INTEGER) [UNIVERSAL 2] matching 0 against ? end "count_C_MSB_DL" of type COUNT_C_MSB begin "count_C_LSB_DL" of type RLC_SequenceNumber (INTEGER) [UNIVERSAL 2] matching 0 against ? end "count_C_LSB_DL" of type RLC_SequenceNumber end "car_GetRLC_SeqNum" of type CRLC_SequenceNumber_CNF Assignment:[9] tcv_RLC_SeqNumDL_RB4 := 0 Receive event:[9] CRLC ? CRLC_SequenceNumber_CNF = PDU (view PDU) Attach:[17] Exit Test Step ts_CRLC_GetRLC_SeqNumSecurity
Attach:[18] Enter Test Step ts_RRC_Security::lt_AssignRB_ActivationTimeInfoList( 0 )
| Assignment:[102] tcv_RB_ActivationTimeInfoList := (view Assignment) Attach:[18] Exit Test Step ts_RRC_Security::lt_AssignRB_ActivationTimeInfoList
Attach:[19] Enter Test Step ts_CRLC_SuspendSecurity( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
00:00:32.250 - Primitive: CRLC_Suspend_REQ Send event:[2] CRLC ! CRLC_Suspend_REQ = PDU: { cellId: -1 , routingInfo: [rB_Identity: 1 ], n: 0 } 00:00:32.290 - Primitive: CRLC_Suspend_CNF begin "car_SuspendRB" of type CRLC_Suspend_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "vt" of type RLC_SequenceNumber (INTEGER) [UNIVERSAL 2] matching 0 against ? end "vt" of type RLC_SequenceNumber end "car_SuspendRB" of type CRLC_Suspend_CNF Receive event:[3] CRLC ? CRLC_Suspend_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 1 ], vt: 0 } 00:00:32.290 - Primitive: CRLC_Suspend_REQ Send event:[4] CRLC ! CRLC_Suspend_REQ = PDU: { cellId: -1 , routingInfo: [rB_Identity: 3 ], n: 3 } 00:00:32.320 - Primitive: CRLC_Suspend_CNF begin "car_SuspendRB" of type CRLC_Suspend_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "vt" of type RLC_SequenceNumber (INTEGER) [UNIVERSAL 2] matching 3 against ? end "vt" of type RLC_SequenceNumber end "car_SuspendRB" of type CRLC_Suspend_CNF Receive event:[5] CRLC ? CRLC_Suspend_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 3 ], vt: 3 } 00:00:32.320 - Primitive: CRLC_Suspend_REQ Send event:[6] CRLC ! CRLC_Suspend_REQ = PDU: { cellId: -1 , routingInfo: [rB_Identity: 4 ], n: 0 } 00:00:32.350 - Primitive: CRLC_Suspend_CNF begin "car_SuspendRB" of type CRLC_Suspend_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "vt" of type RLC_SequenceNumber (INTEGER) [UNIVERSAL 2] matching 0 against ? end "vt" of type RLC_SequenceNumber end "car_SuspendRB" of type CRLC_Suspend_CNF Receive event:[7] CRLC ? CRLC_Suspend_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 4 ], vt: 0 } Attach:[19] Exit Test Step ts_CRLC_SuspendSecurity
Attach:[20] Enter Test Step ts_CRLC_DL_CipherCfgSRB( [startRestart: uea0] )
| Attach:[1] Enter Test Step ts_CRLC_DL_CipherCfgSRB::lt_RLC_Activate( 1 )
| 00:00:32.350 - Primitive: CRLC_Ciphering_Activate_REQ Send event:[5] CRLC ! CRLC_Ciphering_Activate_REQ = PDU (view PDU) 00:00:32.360 - Primitive: CRLC_Ciphering_Activate_CNF begin "ca_CRLC_CipherActCnf" of type CRLC_Ciphering_Activate_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER end "ca_CRLC_CipherActCnf" of type CRLC_Ciphering_Activate_CNF Receive event:[6] CRLC ? CRLC_Ciphering_Activate_CNF = PDU: { cellId: -1 } Attach:[1] Exit Test Step ts_CRLC_DL_CipherCfgSRB::lt_RLC_Activate
Attach:[2] Enter Test Step ts_CRLC_DL_CipherCfgSRB::lt_RLC_Activate( 2 )
| 00:00:32.360 - Primitive: CRLC_Ciphering_Activate_REQ Send event:[5] CRLC ! CRLC_Ciphering_Activate_REQ = PDU (view PDU) 00:00:32.380 - Primitive: CRLC_Ciphering_Activate_CNF begin "ca_CRLC_CipherActCnf" of type CRLC_Ciphering_Activate_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER end "ca_CRLC_CipherActCnf" of type CRLC_Ciphering_Activate_CNF Receive event:[6] CRLC ? CRLC_Ciphering_Activate_CNF = PDU: { cellId: -1 } Attach:[2] Exit Test Step ts_CRLC_DL_CipherCfgSRB::lt_RLC_Activate
Attach:[3] Enter Test Step ts_CRLC_DL_CipherCfgSRB::lt_RLC_Activate( 3 )
| 00:00:32.380 - Primitive: CRLC_Ciphering_Activate_REQ Send event:[5] CRLC ! CRLC_Ciphering_Activate_REQ = PDU (view PDU) 00:00:32.390 - Primitive: CRLC_Ciphering_Activate_CNF begin "ca_CRLC_CipherActCnf" of type CRLC_Ciphering_Activate_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER end "ca_CRLC_CipherActCnf" of type CRLC_Ciphering_Activate_CNF Receive event:[6] CRLC ? CRLC_Ciphering_Activate_CNF = PDU: { cellId: -1 } Attach:[3] Exit Test Step ts_CRLC_DL_CipherCfgSRB::lt_RLC_Activate
Attach:[4] Enter Test Step ts_CRLC_DL_CipherCfgSRB::lt_RLC_Activate( 4 )
| 00:00:32.390 - Primitive: CRLC_Ciphering_Activate_REQ Send event:[5] CRLC ! CRLC_Ciphering_Activate_REQ = PDU (view PDU) 00:00:32.410 - Primitive: CRLC_Ciphering_Activate_CNF begin "ca_CRLC_CipherActCnf" of type CRLC_Ciphering_Activate_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER end "ca_CRLC_CipherActCnf" of type CRLC_Ciphering_Activate_CNF Receive event:[6] CRLC ? CRLC_Ciphering_Activate_CNF = PDU: { cellId: -1 } Attach:[4] Exit Test Step ts_CRLC_DL_CipherCfgSRB::lt_RLC_Activate
Attach:[20] Exit Test Step ts_CRLC_DL_CipherCfgSRB
Attach:[21] Enter Test Step ts_CRLC_DL_CipherCfgRB( [startRestart: uea0] )
| Attach:[21] Exit Test Step ts_CRLC_DL_CipherCfgRB
Attach:[22] Enter Test Step ts_CMAC_CipherCfg( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Preliminary verdict:[6] (PASS) Attach:[22] Exit Test Step ts_CMAC_CipherCfg
Attach:[4] Exit Test Step ts_RRC_Security::lt_ActivateSecurity_DL_SS
Attach:[5] Enter Test Step ts_RRC_Security::lt_RB2_UL_IntegrityActivate( 0 )
| Attach:[13] Enter Test Step ts_RB2_UL_IntegrityActivate( 0 )
| 00:00:32.410 - Primitive: CRLC_Integrity_Activate_REQ Send event:[1] CRLC ! CRLC_Integrity_Activate_REQ = PDU (view PDU) 00:00:32.430 - Primitive: CRLC_Integrity_Activate_CNF begin "ca_CRLC_IntegrityActivateCnf" of type CRLC_Integrity_Activate_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER end "ca_CRLC_IntegrityActivateCnf" of type CRLC_Integrity_Activate_CNF Receive event:[2] CRLC ? CRLC_Integrity_Activate_CNF = PDU: { cellId: -1 } Attach:[13] Exit Test Step ts_RB2_UL_IntegrityActivate
Attach:[5] Exit Test Step ts_RRC_Security::lt_RB2_UL_IntegrityActivate
Attach:[6] Enter Test Step ts_RRC_Security::lt_StartSecurity_UE( 0 )
| Attach:[27] Enter Test Step ts_RRC_Security::lt_SendSecurityModeCommand( 0 )
| 00:00:32.430 - Primitive: RLC_AM_DATA_REQ 00:00:32.430 - Primitive: RLC_AM_DATA_REQ: securityModeCommand Send event:[50] AM ! RLC_AM_DATA_REQ = PDU (view PDU) Attach:[27] Exit Test Step ts_RRC_Security::lt_SendSecurityModeCommand
00:00:32.820 - Primitive: RLC_AM_DATA_IND: securityModeComplete 00:00:32.820 - Primitive: RLC_AM_DATA_IND begin "car_RRC_SecModeCmpl" of type RLC_AM_DATA_IND (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "integrityResult" of type IntegrityResult (CHOICE) [UNIVERSAL 31] matching [integrityUsed: i_pass] against * end "integrityResult" of type IntegrityResult begin "aM_message" of type CHOICE [UNIVERSAL 31] begin "uL_DCCH_Message" of type UL_DCCH_Message (SEQUENCE) [UNIVERSAL 16] begin "integrityCheckInfo" of type IntegrityCheckInfo (SEQUENCE) [UNIVERSAL 16] matching { messageAuthenticationCode: '00001110011110111110000111111100'B , rrc_MessageSequenceNumber: 1 } against * end "integrityCheckInfo" of type IntegrityCheckInfo begin "message" of type UL_DCCH_MessageType (CHOICE) [UNIVERSAL 31] begin "securityModeComplete" of type SecurityModeComplete (SEQUENCE) [UNIVERSAL 16] begin "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier (INTEGER) [UNIVERSAL 2] matching 0 against 0 end "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier begin "ul_IntegProtActivationInfo" of type IntegrityProtActivationInfo (SEQUENCE) [UNIVERSAL 16] matching { rrc_MessageSequenceNumberList: [ 0 , 0 , 0 , 0 , 0 ] } against * end "ul_IntegProtActivationInfo" of type IntegrityProtActivationInfo begin "rb_UL_CiphActivationTimeInfo" of type RB_ActivationTimeInfoList (SEQUENCEOF) [UNIVERSAL 28] matching [ { rb_Identity: 1 , rlc_SequenceNumber: 0 } , { rb_Identity: 2 , rlc_SequenceNumber: 7 } , { rb_Identity: 3 , rlc_SequenceNumber: 4 } , { rb_Identity: 4 , rlc_SequenceNumber: 0 } ] against ? end "rb_UL_CiphActivationTimeInfo" of type RB_ActivationTimeInfoList end "securityModeComplete" of type SecurityModeComplete end "message" of type UL_DCCH_MessageType end "uL_DCCH_Message" of type UL_DCCH_Message end "aM_message" of type CHOICE end "car_RRC_SecModeCmpl" of type RLC_AM_DATA_IND Assignment:TSP1: [29] uL_Integrity := { rrc_MessageSequenceNumberList: [ 0 , 0 , 0 , 0 , 0 ] } Assignment:TSP1: [29] uL_CipherMode := (view Assignment) Receive event:TSP1: [29] AM ? RLC_AM_DATA_IND = PDU (view PDU) Preliminary verdict:TSP1: [29] (PASS) Attach:[30] Enter Test Step ts_CRLC_UL_CipherCfg( [ { rb_Identity: 1 , r ...
| (view Test Step parameters) 00:00:32.820 - Primitive: CRLC_Ciphering_Activate_REQ Send event:[1] CRLC ! CRLC_Ciphering_Activate_REQ = PDU (view PDU) 00:00:33.180 - Primitive: CRLC_Ciphering_Activate_CNF begin "ca_CRLC_CipherActCnf" of type CRLC_Ciphering_Activate_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER end "ca_CRLC_CipherActCnf" of type CRLC_Ciphering_Activate_CNF Receive event:[2] CRLC ? CRLC_Ciphering_Activate_CNF = PDU: { cellId: -1 } Attach:[30] Exit Test Step ts_CRLC_UL_CipherCfg
Attach:[31] Enter Test Step ts_CRLC_UL_Integrity( { rrc_MessageSequenceNumberList: [ 0 , 0 , 0 , 0 , 0 ] } )
| 00:00:33.180 - Primitive: CRLC_Integrity_Activate_REQ Send event:[1] CRLC ! CRLC_Integrity_Activate_REQ = PDU (view PDU) 00:00:33.190 - Primitive: CRLC_Integrity_Activate_CNF begin "ca_CRLC_IntegrityActivateCnf" of type CRLC_Integrity_Activate_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER end "ca_CRLC_IntegrityActivateCnf" of type CRLC_Integrity_Activate_CNF Receive event:[2] CRLC ? CRLC_Integrity_Activate_CNF = PDU: { cellId: -1 } Attach:[31] Exit Test Step ts_CRLC_UL_Integrity
Attach:[6] Exit Test Step ts_RRC_Security::lt_StartSecurity_UE
Attach:[8] Enter Test Step ts_CRLC_ResumeSecurity( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
00:00:33.190 - Primitive: CRLC_Resume_REQ Send event:[2] CRLC ! CRLC_Resume_REQ = PDU: { cellId: -1 , routingInfo: [rB_Identity: 1 ]} 00:00:33.220 - Primitive: CRLC_Resume_CNF begin "car_ResumeRB" of type CRLC_Resume_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "car_ResumeRB" of type CRLC_Resume_CNF Receive event:[3] CRLC ? CRLC_Resume_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 1 ]} 00:00:33.220 - Primitive: CRLC_Resume_REQ Send event:[4] CRLC ! CRLC_Resume_REQ = PDU: { cellId: -1 , routingInfo: [rB_Identity: 3 ]} 00:00:33.250 - Primitive: CRLC_Resume_CNF begin "car_ResumeRB" of type CRLC_Resume_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "car_ResumeRB" of type CRLC_Resume_CNF Receive event:[5] CRLC ? CRLC_Resume_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 3 ]} 00:00:33.250 - Primitive: CRLC_Resume_REQ Send event:[6] CRLC ! CRLC_Resume_REQ = PDU: { cellId: -1 , routingInfo: [rB_Identity: 4 ]} 00:00:33.290 - Primitive: CRLC_Resume_CNF begin "car_ResumeRB" of type CRLC_Resume_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "car_ResumeRB" of type CRLC_Resume_CNF Assignment:[7] tcv_RB_SigResumed := GcTRUE Receive event:[7] CRLC ? CRLC_Resume_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 4 ]} Attach:[8] Exit Test Step ts_CRLC_ResumeSecurity
Attach:[24] Exit Test Step ts_RRC_Security
00:00:33.290 - Primitive: RRC_DATA_REQ: mm:locationUpdatingAccept 00:00:33.290 - Primitive: RLC_AM_DATA_REQ:downlinkDirectTransfer Send event:[25] Dc ! RRC_DataReq = PDU (view PDU) 00:00:33.620 - Primitive: RLC_AM_DATA_IND: uplinkDirectTransfer 00:00:33.620 - Primitive: RRC_DATA_IND: mm:tmsiReallocationComplete begin "car_UplinkDirectTransfer" of type RRC_DataInd (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "rB_Id" of type SS_RB_Identity (INTEGER) [UNIVERSAL 2] matching 3 against 3 end "rB_Id" of type SS_RB_Identity begin "cN_Domain" of type SS_CN_DomainIdentity (INTEGER) [UNIVERSAL 2] matching 0 against 0 end "cN_Domain" of type SS_CN_DomainIdentity begin "msg" of type TMSIREALLOCATIONCOMPLETE (SEQUENCE) [UNIVERSAL 16] begin "skipIndicator" of type SkipIndicator (BITSTRING) [UNIVERSAL 3] matching '0000'B against '0000'B end "skipIndicator" of type SkipIndicator begin "mMProtocolDiscriminator" of type ProtocolDiscriminator (BITSTRING) [UNIVERSAL 3] matching '0101'B against '0101'B end "mMProtocolDiscriminator" of type ProtocolDiscriminator begin "msgType" of type MsgType (BITSTRING) [UNIVERSAL 3] matching '10011011'B against '??011011'B end "msgType" of type MsgType end "msg" of type TMSIREALLOCATIONCOMPLETE end "car_UplinkDirectTransfer" of type RRC_DataInd Receive event:[26] Dc ? RRC_DataInd = PDU (view PDU) Attach:[27] Enter Test Step ts_GMM_IdleUpdated::lt_RRC_ConnRel( 0 )
| Attach:[120] Enter Test Step ts_RRC_ConnRel( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[2] Enter Test Step ts_RRC_Delay( 1000 )
| StartTimer:[1] t_Dly [5000] 1000 ms Timed out Timer:t_Dly TimeOut:[2] t_Dly [5000] 1000 ms Attach:[2] Exit Test Step ts_RRC_Delay
Attach:[3] Enter Test Step ts_RRC_ConnRel::lt_Send_RRC_ConnectionRelease( 0 )
| Assignment:[39] tcv_N308 := 1 Assignment:[39] tcv_K := 1 00:00:34.660 - Primitive: RLC_UM_DATA_REQ 00:00:34.660 - Primitive: RLC_UM_DATA_REQ: rrcConnectionRelease Send event:[40] UM ! RLC_UM_DATA_REQ = PDU (view PDU) 00:00:35.050 - Primitive: RLC_UM_DATA_IND: rrcConnectionReleaseComplete 00:00:35.050 - Primitive: RLC_UM_DATA_IND begin "car_RRC_ConnRelCmplUM" of type RLC_UM_DATA_IND (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "integrityResult" of type IntegrityResult (CHOICE) [UNIVERSAL 31] matching [integrityUsed: i_pass] against * end "integrityResult" of type IntegrityResult begin "uM_message" of type CHOICE [UNIVERSAL 31] begin "uL_DCCH_Message" of type UL_DCCH_Message (SEQUENCE) [UNIVERSAL 16] begin "integrityCheckInfo" of type IntegrityCheckInfo (SEQUENCE) [UNIVERSAL 16] matching { messageAuthenticationCode: '11110111111000101100001011001110'B , rrc_MessageSequenceNumber: 1 } against * end "integrityCheckInfo" of type IntegrityCheckInfo begin "message" of type UL_DCCH_MessageType (CHOICE) [UNIVERSAL 31] begin "rrcConnectionReleaseComplete" of type RRCConnectionReleaseComplete (SEQUENCE) [UNIVERSAL 16] begin "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier (INTEGER) [UNIVERSAL 2] matching 0 against 0 end "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier end "rrcConnectionReleaseComplete" of type RRCConnectionReleaseComplete end "message" of type UL_DCCH_MessageType end "uL_DCCH_Message" of type UL_DCCH_Message end "uM_message" of type CHOICE end "car_RRC_ConnRelCmplUM" of type RLC_UM_DATA_IND Receive event:TSP1: [41] UM ? RLC_UM_DATA_IND = PDU (view PDU) Preliminary verdict:TSP1: [41] (PASS) Attach:[42] Enter Test Step ts_RRC_ConnRel::lt_RptRcvConnRel( 0 )
| StartTimer:[49] t_Dly [5000] 5000 ms 00:00:35.220 - Primitive: RLC_UM_DATA_IND: rrcConnectionReleaseComplete 00:00:35.220 - Primitive: RLC_UM_DATA_IND begin "car_RRC_ConnRelCmplUM" of type RLC_UM_DATA_IND (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "integrityResult" of type IntegrityResult (CHOICE) [UNIVERSAL 31] matching [integrityUsed: i_pass] against * end "integrityResult" of type IntegrityResult begin "uM_message" of type CHOICE [UNIVERSAL 31] begin "uL_DCCH_Message" of type UL_DCCH_Message (SEQUENCE) [UNIVERSAL 16] begin "integrityCheckInfo" of type IntegrityCheckInfo (SEQUENCE) [UNIVERSAL 16] matching { messageAuthenticationCode: '10111001101000110000011111000000'B , rrc_MessageSequenceNumber: 2 } against * end "integrityCheckInfo" of type IntegrityCheckInfo begin "message" of type UL_DCCH_MessageType (CHOICE) [UNIVERSAL 31] begin "rrcConnectionReleaseComplete" of type RRCConnectionReleaseComplete (SEQUENCE) [UNIVERSAL 16] begin "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier (INTEGER) [UNIVERSAL 2] matching 0 against 0 end "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier end "rrcConnectionReleaseComplete" of type RRCConnectionReleaseComplete end "message" of type UL_DCCH_MessageType end "uL_DCCH_Message" of type UL_DCCH_Message end "uM_message" of type CHOICE end "car_RRC_ConnRelCmplUM" of type RLC_UM_DATA_IND Assignment:TSP2: [52] tcv_K := 2 CancelTimer:TSP2: [52] t_Dly [5000] 5000 ms Receive event:TSP2: [52] UM ? RLC_UM_DATA_IND = PDU (view PDU) Preliminary verdict:TSP2: [52] (PASS) Attach:[42] Exit Test Step ts_RRC_ConnRel::lt_RptRcvConnRel
Attach:[3] Exit Test Step ts_RRC_ConnRel::lt_Send_RRC_ConnectionRelease
Attach:[4] Enter Test Step ts_RRC_ConnRel::lt_RestartCRLC_ForNextConnection( 0 )
| Attach:[7] Enter Test Step ts_CRLC_RelReconfSRB( 0 )
| Attach:[1] Enter Test Step ts_CRLC_Rel( -1 )
| 00:00:35.220 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:00:35.290 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 1 ]} Attach:[1] Exit Test Step ts_CRLC_Rel
Attach:[2] Enter Test Step ts_CRLC_Rel( -1 )
| 00:00:35.290 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:00:35.330 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 2 ]} Attach:[2] Exit Test Step ts_CRLC_Rel
Attach:[3] Enter Test Step ts_CRLC_Rel( -1 )
| 00:00:35.330 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:00:35.440 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 3 ]} Attach:[3] Exit Test Step ts_CRLC_Rel
Attach:[4] Enter Test Step ts_CRLC_Rel( -1 )
| 00:00:35.440 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:00:35.550 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 4 ]} Attach:[4] Exit Test Step ts_CRLC_Rel
Attach:[5] Enter Test Step ts_SS_RB1_ToRB4_Cfg( )
| 00:00:35.550 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:00:35.600 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 1 ]} 00:00:35.600 - Primitive: CRLC_Config_REQ Send event:[3] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:00:35.770 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[4] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 2 ]} 00:00:35.770 - Primitive: CRLC_Config_REQ Send event:[5] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:00:35.940 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[6] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 3 ]} 00:00:35.940 - Primitive: CRLC_Config_REQ Send event:[7] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:00:35.990 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[8] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 4 ]} Attach:[5] Exit Test Step ts_SS_RB1_ToRB4_Cfg
Attach:[7] Exit Test Step ts_CRLC_RelReconfSRB
Attach:[8] Enter Test Step ts_SetCellCfg( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Assignment:[2] cellConfig := cell_DCH_StandAloneSRB_NoConn Attach:[3] Enter Test Step ts_SaveCellInfo( 0 )
| Assignment:[2] tcv_CellInfoA := (view Assignment) Attach:[3] Exit Test Step ts_SaveCellInfo
Attach:[8] Exit Test Step ts_SetCellCfg
Attach:[4] Exit Test Step ts_RRC_ConnRel::lt_RestartCRLC_ForNextConnection
Attach:[5] Enter Test Step ts_SS_ResetSecurityKey( )
| Assignment:[1] tcv_CellIndInfo := (view Assignment) Assignment:[5] cipheringAlgorithmCapability := '0000000000000001'B Attach:[5] Exit Test Step ts_SS_ResetSecurityKey
Attach:[120] Exit Test Step ts_RRC_ConnRel
Attach:[27] Exit Test Step ts_GMM_IdleUpdated::lt_RRC_ConnRel
StartTimer:[28] t_WaitS [15] 1 s Timed out Timer:t_WaitS TimeOut:[29] t_WaitS [15] 1 s StartTimer:[30] t_WaitS [15] 60 s Attach:[31] Enter Test Step ts_AT_TriggerGMM_Attach( )
| 00:00:37.000 - Primitive: AT_CmdReq Send event:[1] Ut ! AT_CmdReq = PDU: { cmd: "AT+CGATT=1<CR>" , sMS_BlockMode: OMIT} 00:01:26.520 - Primitive: RLC_TR_DATA_IND: rrcConnectionRequest 00:01:26.520 - Primitive: RLC_TR_DATA_IND 00:01:28.290 - Primitive: AT_CmdCnf begin "ca_AT_CmdCnf" of type AT_CmdCnf (SEQUENCE) [UNIVERSAL 16] begin "resultString" of type IA5String [UNIVERSAL 22] matching "<CR><LF>OK<CR><LF>" against "<CR><LF>OK<CR><LF>" IF PRESENT end "resultString" of type IA5String end "ca_AT_CmdCnf" of type AT_CmdCnf Receive event:[2] Ut ? AT_CmdCnf = PDU (view PDU) Attach:[31] Exit Test Step ts_AT_TriggerGMM_Attach
Attach:[32] Enter Test Step ts_RRC_ConnEst( 0 )
| Attach:[1] Enter Test Step ts_SS_PrepareCellRRC_ConnEst( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[1] Exit Test Step ts_SS_PrepareCellRRC_ConnEst
Attach:[2] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[2] Exit Test Step ts_SetTmpCellInfo
Attach:[3] Enter Test Step ts_RRC_ConnEst::lt_RcvConnReq( 0 )
| begin "car_RRC_ConnReq" of type RLC_TR_DATA_IND (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "tM_message" of type CHOICE [UNIVERSAL 31] begin "uL_CCCH_Message" of type UL_CCCH_Message (SEQUENCE) [UNIVERSAL 16] begin "message" of type UL_CCCH_MessageType (CHOICE) [UNIVERSAL 31] begin "rrcConnectionRequest" of type RRCConnectionRequest (SEQUENCE) [UNIVERSAL 16] begin "initialUE_Identity" of type InitialUE_Identity (CHOICE) [UNIVERSAL 31] begin InitialUE_Identity (CHOICE) [UNIVERSAL 31] end InitialUE_Identity begin InitialUE_Identity (CHOICE) [UNIVERSAL 31] begin "tmsi_and_LAI" of type TMSI_and_LAI_GSM_MAP (SEQUENCE) [UNIVERSAL 16] matching { tmsi: '00010001001000100011001101000100'B , lai: { plmn_Identity: { mcc: [ 0 , 0 , 1 ] , mnc: [ 0 , 1 ] } , lac: '0000000000000001'B } } against ? end "tmsi_and_LAI" of type TMSI_and_LAI_GSM_MAP end InitialUE_Identity matching [tmsi_and_LAI: { tmsi: '00010001001000100011001101000100'B , lai: { plmn_Identity: { mcc: [ 0 , 0 , 1 ] , mnc: [ 0 , 1 ] } , lac: '0000000000000001'B } } ] against ([imsi: ?], [tmsi_and_LAI: ?], [p_TMSI_and_RAI: ?], [imei: ?]) end "initialUE_Identity" of type InitialUE_Identity begin "establishmentCause" of type EstablishmentCause (ENUMERATED) [UNIVERSAL 10] matching registration against registration end "establishmentCause" of type EstablishmentCause begin "protocolErrorIndicator" of type ProtocolErrorIndicator (ENUMERATED) [UNIVERSAL 10] matching noError against noError end "protocolErrorIndicator" of type ProtocolErrorIndicator end "rrcConnectionRequest" of type RRCConnectionRequest end "message" of type UL_CCCH_MessageType end "uL_CCCH_Message" of type UL_CCCH_Message end "tM_message" of type CHOICE end "car_RRC_ConnReq" of type RLC_TR_DATA_IND Assignment:[7] tcv_InitialUE_Id := (view Assignment) Receive event:[7] TM ? RLC_TR_DATA_IND = PDU (view PDU) Attach:[3] Exit Test Step ts_RRC_ConnEst::lt_RcvConnReq
Attach:[4] Enter Test Step ts_RRC_ConnEst::lt_Send_ConnSetUp( 0 )
| 00:01:28.290 - Primitive: RLC_UM_DATA_REQ 00:01:28.290 - Primitive: RLC_UM_DATA_REQ: rrcConnectionSetup Send event:[31] UM ! RLC_UM_DATA_REQ = PDU (view PDU) Attach:[33] Enter Test Step ts_SetCellCfg( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Assignment:[2] cellConfig := cell_DCH_StandAloneSRB Attach:[3] Enter Test Step ts_SaveCellInfo( 0 )
| Assignment:[2] tcv_CellInfoA := (view Assignment) Attach:[3] Exit Test Step ts_SaveCellInfo
Attach:[33] Exit Test Step ts_SetCellCfg
Attach:[4] Exit Test Step ts_RRC_ConnEst::lt_Send_ConnSetUp
Attach:[5] Enter Test Step ts_RRC_ReceiveConnSetupCmpl( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
StartTimer:[3] t_WaitMS [13500] 13500 ms 00:01:28.890 - Primitive: RLC_AM_DATA_IND: rrcConnectionSetupComplete 00:01:28.910 - Primitive: RLC_AM_DATA_IND begin "car_RRC_ConnSetupCmpl" of type RLC_AM_DATA_IND (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "integrityResult" of type IntegrityResult (CHOICE) [UNIVERSAL 31] matching [integrityUsed: i_pass] against ? end "integrityResult" of type IntegrityResult begin "aM_message" of type CHOICE [UNIVERSAL 31] begin "uL_DCCH_Message" of type UL_DCCH_Message (SEQUENCE) [UNIVERSAL 16] begin "message" of type UL_DCCH_MessageType (CHOICE) [UNIVERSAL 31] begin "rrcConnectionSetupComplete" of type RRCConnectionSetupComplete (SEQUENCE) [UNIVERSAL 16] begin "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier (INTEGER) [UNIVERSAL 2] matching 0 against 0 end "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier begin "startList" of type STARTList (SEQUENCEOF) [UNIVERSAL 28] matching [ { cn_DomainIdentity: ps_domain, start_Value: '00000000000000000010'B } , { cn_DomainIdentity: cs_domain, start_Value: '00000000000000000010'B } ] against ? end "startList" of type STARTList begin "ue_RadioAccessCapability" of type UE_RadioAccessCapability (SEQUENCE) [UNIVERSAL 16] matching { accessStratumReleaseIndicator: r99, pdcp_Capability: { losslessSRNS_RelocationSupport: GcTRUE , supportForRfc2507: [supported: by8192]} , rlc_Capability: { totalRLC_AM_BufferSize: kb50, maximumRLC_WindowSize: mws2047, maximumAM_EntityNumber: am6} , transportChannelCapability: { dl_TransChCapability: { maxNoBitsReceived: b5120, maxConvCodeBitsReceived: b1280, turboDecodingSupport: [supported: b5120], maxSimultaneousTransChs: e8, maxSimultaneousCCTrCH_Count: 1 , maxReceivedTransportBlocks: tb16, maxNumberOfTFC: tfc96, maxNumberOfTF: tf64} , ul_TransChCapability: { maxNoBitsTransmitted: b3840, maxConvCodeBitsTransmitted: b1280, turboEncodingSupport: [supported: b3840], maxSimultaneousTransChs: e8, modeSpecificInfo: [fdd: NULL], maxTransmittedBlocks: tb8, maxNumberOfTFC: tfc32, maxNumberOfTF: tf32} } , rf_Capability: { fddRF_Capability: { ue_PowerClass: 4 , txRxFrequencySeparation: mhz190} , tddRF_Capability: OMIT} , physicalChannelCapability: { fddPhysChCapability: { downlinkPhysChCapability: { maxNoDPCH_PDSCH_Codes: 3 , maxNoPhysChBitsReceived: b9600, supportForSF_512: GcFALSE , supportOfPDSCH: GcFALSE , simultaneousSCCPCH_DPCH_Reception: [notSupported: NULL]} , uplinkPhysChCapability: { maxNoDPDCH_BitsTransmitted: b2400, supportOfPCPCH: GcFALSE } } , tddPhysChCapability: OMIT} , ue_MultiModeRAT_Capability: { multiRAT_CapabilityList: { supportOfGSM: GcFALSE , supportOfMulticarrier: GcFALSE } , multiModeCapability: fdd} , securityCapability: { cipheringAlgorithmCap: '0000000000000001'B , integrityProtectionAlgorithmCap: '0000000000000010'B } , ue_positioning_Capability: { standaloneLocMethodsSupported: GcFALSE , ue_BasedOTDOA_Supported: GcFALSE , networkAssistedGPS_Supported: noNetworkAssistedGPS, supportForUE_GPS_TimingOfCellFrames: GcFALSE , supportForIPDL: GcFALSE } , measurementCapability: { downlinkCompressedMode: { fdd_Measurements: GcTRUE , tdd_Measurements: OMIT, gsm_Measurements: { gsm900: GcTRUE , dcs1800: GcTRUE , gsm1900: GcFALSE } , multiCarrierMeasurements: GcFALSE } , uplinkCompressedMode: { fdd_Measurements: GcTRUE , tdd_Measurements: OMIT, gsm_Measurements: { gsm900: GcTRUE , dcs1800: GcTRUE , gsm1900: GcFALSE } , multiCarrierMeasurements: GcFALSE } } } against * end "ue_RadioAccessCapability" of type UE_RadioAccessCapability end "rrcConnectionSetupComplete" of type RRCConnectionSetupComplete end "message" of type UL_DCCH_MessageType end "uL_DCCH_Message" of type UL_DCCH_Message end "aM_message" of type CHOICE end "car_RRC_ConnSetupCmpl" of type RLC_AM_DATA_IND Assignment:TSP1: [5] tcv_StartList := (view Assignment) Assignment:TSP1: [5] cipheringAlgorithmCapability := '0000000000000001'B CancelTimer:TSP1: [5] t_WaitMS [13500] 13500 ms Receive event:TSP1: [5] AM ? RLC_AM_DATA_IND = PDU (view PDU) Preliminary verdict:TSP1: [5] (PASS) Attach:[6] Enter Test Step ts_RRC_ReceiveConnSetupCmpl::lt_GetHFN( 0 )
| Assignment:[13] tcv_Count := 2 Attach:[17] Enter Test Step ts_RRC_ReceiveConnSetupCmpl::lt_FirstValue( 0 )
| Assignment:[23] start_PS := '00000000000000000010'B Attach:[17] Exit Test Step ts_RRC_ReceiveConnSetupCmpl::lt_FirstValue
Attach:[18] Enter Test Step ts_RRC_ReceiveConnSetupCmpl::lt_SecondValue( 0 )
| Assignment:[26] start_CS := '00000000000000000010'B Attach:[18] Exit Test Step ts_RRC_ReceiveConnSetupCmpl::lt_SecondValue
Attach:[6] Exit Test Step ts_RRC_ReceiveConnSetupCmpl::lt_GetHFN
Attach:[5] Exit Test Step ts_RRC_ReceiveConnSetupCmpl
Attach:[32] Exit Test Step ts_RRC_ConnEst
00:01:28.900 - Primitive: RLC_AM_DATA_IND: initialDirectTransfer 00:01:28.900 - Primitive: RRC_DATA_IND: gmm:attachRequest begin "car_PS_InitDirectTransfer" of type RRC_DataInd (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "rB_Id" of type SS_RB_Identity (INTEGER) [UNIVERSAL 2] matching 3 against 3 end "rB_Id" of type SS_RB_Identity begin "cN_Domain" of type SS_CN_DomainIdentity (INTEGER) [UNIVERSAL 2] matching 1 against 1 end "cN_Domain" of type SS_CN_DomainIdentity begin "start" of type START_Value (BITSTRING) [UNIVERSAL 3] matching '00000000000000000010'B against ? end "start" of type START_Value begin "msg" of type ATTACHREQUEST (SEQUENCE) [UNIVERSAL 16] begin "skipIndicator" of type SkipIndicator (BITSTRING) [UNIVERSAL 3] matching '0000'B against '0000'B end "skipIndicator" of type SkipIndicator begin "gMMProtocolDiscriminator" of type ProtocolDiscriminator (BITSTRING) [UNIVERSAL 3] matching '1000'B against '1000'B end "gMMProtocolDiscriminator" of type ProtocolDiscriminator begin "msgType" of type MsgType (BITSTRING) [UNIVERSAL 3] matching '00000001'B against '00000001'B end "msgType" of type MsgType begin "msNetworkCap" of type MS_NetworkCap_lv (SEQUENCE) [UNIVERSAL 16] matching { iel: '02'O , value: 'E540'O } against ? end "msNetworkCap" of type MS_NetworkCap_lv begin "gprsCiphKeySeqNo" of type CiphKeySeqNum (SEQUENCE) [UNIVERSAL 16] begin "spare1" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against '0'B end "spare1" of type B1 begin "keySeq" of type KeySeq (BITSTRING) [UNIVERSAL 3] matching '000'B against ? end "keySeq" of type KeySeq end "gprsCiphKeySeqNo" of type CiphKeySeqNum begin "attachType" of type AttachType (SEQUENCE) [UNIVERSAL 16] begin "for" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against ? end "for" of type B1 begin "type" of type B3 (BITSTRING) [UNIVERSAL 3] matching '011'B against ? end "type" of type B3 end "attachType" of type AttachType begin "drxParameter" of type DRXparamter (SEQUENCE) [UNIVERSAL 16] matching { splitPGcycleCode: '00000111'B , cnDRXcoef: '0000'B , splitOnCCCH: '0'B , nonDRXtimer: '010'B } against ? end "drxParameter" of type DRXparamter begin "ptmsiORimsi" of type MS_Identity_lv (SEQUENCE) [UNIVERSAL 16] begin "iel" of type Length (OCTETSTRING) [UNIVERSAL 4] matching '05'O against ? end "iel" of type Length begin "iDigit1" of type B4 (BITSTRING) [UNIVERSAL 3] matching '1111'B against ? end "iDigit1" of type B4 begin "oddEvenInd" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against ? end "oddEvenInd" of type B1 begin "typeOfId" of type B3 (BITSTRING) [UNIVERSAL 3] matching '100'B against ? end "typeOfId" of type B3 begin "otherDigits" of type OCTETSTRING [UNIVERSAL 4] matching '12345678'O against ? end "otherDigits" of type OCTETSTRING end "ptmsiORimsi" of type MS_Identity_lv begin "oldRAI" of type RAI_v (SEQUENCE) [UNIVERSAL 16] begin "plmn" of type OCTETSTRING [UNIVERSAL 4] matching '00F110'O against ? end "plmn" of type OCTETSTRING begin "lac" of type OCTETSTRING [UNIVERSAL 4] matching '0001'O against ? end "lac" of type OCTETSTRING begin "rac" of type OCTETSTRING [UNIVERSAL 4] matching '05'O against ? end "rac" of type OCTETSTRING end "oldRAI" of type RAI_v begin "msRadioAccessCap" of type MSRadioAccessCap_lv (SEQUENCE) [UNIVERSAL 16] matching { iel: '0A'O , value: '14F382334C03263CA060'O } against ? end "msRadioAccessCap" of type MSRadioAccessCap_lv begin "readyTimer" of type GPRS_Timer (SEQUENCE) [UNIVERSAL 16] begin "iei" of type IEI8 (BITSTRING) [UNIVERSAL 3] matching '00010111'B against '00010111'B end "iei" of type IEI8 begin "unit" of type B3 (BITSTRING) [UNIVERSAL 3] matching '000'B against ? end "unit" of type B3 begin "value" of type B5 (BITSTRING) [UNIVERSAL 3] matching '10110'B against ? end "value" of type B5 end "readyTimer" of type GPRS_Timer end "msg" of type ATTACHREQUEST end "car_PS_InitDirectTransfer" of type RRC_DataInd Assignment:[33] tcv_TmpAttachReqPDU (view PDU) Assignment:[33] tcv_TmpB3 := '011'B Assignment:[33] tcv_Start := '00000000000000000010'B CancelTimer:[33] t_WaitS [15] 60 s Receive event:[33] Dc ? RRC_DataInd = PDU (view PDU) Attach:[34] Enter Test Step ts_SS_SecurityDownloadStart( ps_domain )
| Assignment:[4] start_PS := '00000000000000000010'B Attach:[34] Exit Test Step ts_SS_SecurityDownloadStart
Attach:[35] Enter Test Step ts_GMM_Authentication( 0 )
| Attach:[1] Enter Test Step ts_GMM_AuthenticationInit( )
| Attach:[1] Enter Test Step ts_GMM_AuthenticationInit::lt_IncrementCiphKeySeqNum( )
| Assignment:[18] tcv_PS_KeySeq := '000'B Attach:[1] Exit Test Step ts_GMM_AuthenticationInit::lt_IncrementCiphKeySeqNum
Attach:[2] Enter Test Step ts_GMM_AuthenticationInit::lt_AuthCalcAUTN( )
| Assignment:[19] tcv_AuthXDOUT := (view Assignment) Assignment:[20] tcv_AuthCDOUT := '0000000000000000000000000000000000000000000000000000000000000000'B Assignment:[21] tcv_AuthXDOUT_Half := '0101010101000100011101110110011000010001000000000011001100100010'B Assignment:[22] tcv_AuthAK := '011001100001000100000000001100110010001011011101'B Assignment:[23] tcv_AuthAUTN_1 := '011001100001000100000000001100110010001011011101'B Assignment:[24] tcv_AuthMAC := '0101010101000100011101110110011000010001000000000011001100100010'B Assignment:[25] tcv_AuthAUTN_2 := (view Assignment) Assignment:[26] tcv_AuthAUTN := (view Assignment) Attach:[2] Exit Test Step ts_GMM_AuthenticationInit::lt_AuthCalcAUTN
Attach:[3] Enter Test Step ts_GMM_AuthenticationInit::lt_AuthCalcUMTS_Others( )
| Assignment:[27] tcv_PS_AuthIK := (view Assignment) Assignment:[28] tcv_PS_AuthCK := (view Assignment) Assignment:[29] tcv_AuthXRES := (view Assignment) Attach:[3] Exit Test Step ts_GMM_AuthenticationInit::lt_AuthCalcUMTS_Others
Attach:[4] Enter Test Step ts_GMM_AuthenticationInit::lt_AuthCalcKcGSM( )
| Assignment:[30] tcv_AuthCK_1 := '0100010001110111011001100001000100000000001100110010001011011101'B Assignment:[31] tcv_AuthCK_2 := '1100110011111111111011101001100110001000101110111010101001010101'B Assignment:[32] tcv_AuthIK_1 := '0111011101100110000100010000000000110011001000101101110111001100'B Assignment:[33] tcv_AuthIK_2 := '1111111111101110100110011000100010111011101010100101010101000100'B Assignment:[34] tcv_AuthCK_XOR := '1000100010001000100010001000100010001000100010001000100010001000'B Assignment:[35] tcv_AuthIK_XOR := '1000100010001000100010001000100010001000100010001000100010001000'B Assignment:[36] tcv_AuthKcGSM := '0000000000000000000000000000000000000000000000000000000000000000'B Attach:[4] Exit Test Step ts_GMM_AuthenticationInit::lt_AuthCalcKcGSM
Attach:[1] Exit Test Step ts_GMM_AuthenticationInit
00:01:28.930 - Primitive: RRC_DATA_REQ: gmm:authenticationAndCipheringRequest 00:01:28.940 - Primitive: RLC_AM_DATA_REQ:downlinkDirectTransfer Send event:[2] Dc ! RRC_DataReq = PDU (view PDU) 00:01:29.450 - Primitive: RLC_AM_DATA_IND: uplinkDirectTransfer 00:01:29.450 - Primitive: RRC_DATA_IND: gmm:authenticationAndCipheringResponse begin "car_PS_UplinkDirectTransfer" of type RRC_DataInd (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "rB_Id" of type SS_RB_Identity (INTEGER) [UNIVERSAL 2] matching 3 against 3 end "rB_Id" of type SS_RB_Identity begin "cN_Domain" of type SS_CN_DomainIdentity (INTEGER) [UNIVERSAL 2] matching 1 against 1 end "cN_Domain" of type SS_CN_DomainIdentity begin "msg" of type AUTHENTICATIONANDCIPHERINGRESPONSE (SEQUENCE) [UNIVERSAL 16] begin "skipIndicator" of type SkipIndicator (BITSTRING) [UNIVERSAL 3] matching '0000'B against '0000'B end "skipIndicator" of type SkipIndicator begin "gMMProtocolDiscriminator" of type ProtocolDiscriminator (BITSTRING) [UNIVERSAL 3] matching '1000'B against '1000'B end "gMMProtocolDiscriminator" of type ProtocolDiscriminator begin "msgType" of type MsgType (BITSTRING) [UNIVERSAL 3] matching '00010011'B against '00010011'B end "msgType" of type MsgType begin "spare4" of type B4 (BITSTRING) [UNIVERSAL 3] matching '0000'B against '0000'B end "spare4" of type B4 begin "acRefNo" of type AC_ReferenceNumber (SEQUENCE) [UNIVERSAL 16] matching { value: '0011'B } against ? end "acRefNo" of type AC_ReferenceNumber begin "authRsp" of type AuthRsp_tv (SEQUENCE) [UNIVERSAL 16] begin "iei" of type IEI8 (BITSTRING) [UNIVERSAL 3] matching '00100010'B against '00100010'B end "iei" of type IEI8 begin "value" of type BITSTRING [UNIVERSAL 3] matching '01010101010001000111011101100110'B against ? end "value" of type BITSTRING end "authRsp" of type AuthRsp_tv begin "authRspExt" of type AuthRspExt (SEQUENCE) [UNIVERSAL 16] begin "iei" of type IEI8 (BITSTRING) [UNIVERSAL 3] matching '00101001'B against '00101001'B end "iei" of type IEI8 begin "iel" of type Length (OCTETSTRING) [UNIVERSAL 4] matching '0C'O against ? end "iel" of type Length begin "rES" of type BITSTRING [UNIVERSAL 3] matching '000100010000000000110011001000101101110111001100111111111110111010011001100010001011101110101010'B against ? end "rES" of type BITSTRING end "authRspExt" of type AuthRspExt end "msg" of type AUTHENTICATIONANDCIPHERINGRESPONSE end "car_PS_UplinkDirectTransfer" of type RRC_DataInd Assignment:[3] tcv_TmpAuthAndCiphRspPDU (view PDU) Assignment:[3] tcv_AuthRsp := '01010101010001000111011101100110'B Assignment:[3] tcv_AuthRspExt := (view Assignment) Receive event:[3] Dc ? RRC_DataInd = PDU (view PDU) Assignment:[4] tcv_Res := GcTRUE Preliminary verdict:TSP1: [6] (PASS) Attach:[35] Exit Test Step ts_GMM_Authentication
Attach:[36] Enter Test Step ts_GMM_IdleUpdated::lt_SecurityMode( 0 )
| Attach:[100] Enter Test Step ts_RRC_Security( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[2] Enter Test Step ts_RRC_Security::lt_RRC_InitVariables( 0 )
| Attach:[53] Enter Test Step ts_RRC_Security::lt_InitCipherMode( 0 )
| Assignment:[76] dL_CipherMode := [startRestart: uea0] Assignment:[76] cipheringAlgorithmCapability := '0000000000000001'B Assignment:[80] ps_cipheringStarted := GcTRUE Attach:[53] Exit Test Step ts_RRC_Security::lt_InitCipherMode
Attach:[54] Enter Test Step ts_RRC_Security::lt_InitIntegrity( 0 )
| Assignment:[87] recentSecureDomain := ps_domain Assignment:[92] dL_Integrity := (view Assignment) Assignment:[92] integrityStarted := GcTRUE Assignment:[92] dl_IntegrityCheckInfo := (view Assignment) Assignment:[92] tcv_Int_ModifyFlag := GcFALSE Attach:[54] Exit Test Step ts_RRC_Security::lt_InitIntegrity
Attach:[55] Enter Test Step ts_InitSystemSpecificCap( )
| Assignment:[11] tcv_UE_SystemSpecificCap := 0 Attach:[55] Exit Test Step ts_InitSystemSpecificCap
Attach:[56] Enter Test Step ts_SaveCellInfo( 0 )
| Assignment:[2] tcv_CellInfoA := (view Assignment) Attach:[56] Exit Test Step ts_SaveCellInfo
Assignment:[58] tcv_HFN := '00000000000000000000'B Assignment:[62] start_PS := '00000000000000000000'B Attach:[2] Exit Test Step ts_RRC_Security::lt_RRC_InitVariables
Attach:[3] Enter Test Step ts_SS_DownloadSecurityKey( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[6] Enter Test Step ts_SS_DownloadSecurityKey::lt_DownloadKeyCRLC( '00000000000000000000'B )
| 00:01:29.460 - Primitive: CRLC_SecurityMode_Config_REQ 00:01:29.460 - Primitive: CRLC_SecurityMode_Config_REQ Send event:[21] CRLC ! CRLC_SecurityMode_Config_REQ = PDU (view PDU) 00:01:29.470 - Primitive: CRLC_SecurityMode_Config_CNF begin "ca_CRLC_SecurityModeCfgCnf" of type CRLC_SecurityMode_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER end "ca_CRLC_SecurityModeCfgCnf" of type CRLC_SecurityMode_Config_CNF Receive event:[22] CRLC ? CRLC_SecurityMode_Config_CNF = PDU: { cellId: -1 } Attach:[6] Exit Test Step ts_SS_DownloadSecurityKey::lt_DownloadKeyCRLC
Attach:[3] Exit Test Step ts_SS_DownloadSecurityKey
Attach:[4] Enter Test Step ts_RRC_Security::lt_ActivateSecurity_DL_SS( 0 )
| Attach:[14] Enter Test Step ts_RRC_Security::lt_InitialiseRRC_MSN( 0 )
| Attach:[25] Enter Test Step ts_SetDL_RRC_MessageSN( 0 )
| 00:01:29.470 - Primitive: CRLC_SetRRC_MessageSN_REQ Send event:[1] CRLC ! CRLC_SetRRC_MessageSN_REQ = PDU (view PDU) 00:01:29.490 - Primitive: CRLC_SetRRC_MessageSN_CNF begin "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF Receive event:[2] CRLC ? CRLC_SetRRC_MessageSN_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: 0 ]} 00:01:29.490 - Primitive: CRLC_SetRRC_MessageSN_REQ Send event:[3] CRLC ! CRLC_SetRRC_MessageSN_REQ = PDU (view PDU) 00:01:29.500 - Primitive: CRLC_SetRRC_MessageSN_CNF begin "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF Receive event:[4] CRLC ? CRLC_SetRRC_MessageSN_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 1 ]} 00:01:29.500 - Primitive: CRLC_SetRRC_MessageSN_REQ Send event:[5] CRLC ! CRLC_SetRRC_MessageSN_REQ = PDU (view PDU) 00:01:29.520 - Primitive: CRLC_SetRRC_MessageSN_CNF begin "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF Receive event:[6] CRLC ? CRLC_SetRRC_MessageSN_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 2 ]} 00:01:29.520 - Primitive: CRLC_SetRRC_MessageSN_REQ Send event:[7] CRLC ! CRLC_SetRRC_MessageSN_REQ = PDU (view PDU) 00:01:29.540 - Primitive: CRLC_SetRRC_MessageSN_CNF begin "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF Receive event:[8] CRLC ? CRLC_SetRRC_MessageSN_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 3 ]} 00:01:29.540 - Primitive: CRLC_SetRRC_MessageSN_REQ Send event:[9] CRLC ! CRLC_SetRRC_MessageSN_REQ = PDU (view PDU) 00:01:29.550 - Primitive: CRLC_SetRRC_MessageSN_CNF begin "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF Receive event:[10] CRLC ? CRLC_SetRRC_MessageSN_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 4 ]} Attach:[25] Exit Test Step ts_SetDL_RRC_MessageSN
Attach:[14] Exit Test Step ts_RRC_Security::lt_InitialiseRRC_MSN
Attach:[15] Enter Test Step ts_CRLC_DL_Integrity( { integrityProtectionM ...
| (view Test Step parameters) 00:01:29.550 - Primitive: CRLC_Integrity_Activate_REQ 00:01:29.550 - Primitive: CRLC_Integrity_Activate_REQ Send event:[1] CRLC ! CRLC_Integrity_Activate_REQ = PDU (view PDU) 00:01:29.570 - Primitive: CRLC_Integrity_Activate_CNF begin "ca_CRLC_IntegrityActivateCnf" of type CRLC_Integrity_Activate_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER end "ca_CRLC_IntegrityActivateCnf" of type CRLC_Integrity_Activate_CNF Receive event:[2] CRLC ? CRLC_Integrity_Activate_CNF = PDU: { cellId: -1 } Attach:[15] Exit Test Step ts_CRLC_DL_Integrity
Attach:[17] Enter Test Step ts_CRLC_GetRLC_SeqNumSecurity( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
00:01:29.570 - Primitive: CRLC_SequenceNumber_REQ Send event:[2] CRLC ! CRLC_SequenceNumber_REQ = PDU: { cellId: -1 , routingInfo: [rB_Identity: 1 ]} 00:01:29.600 - Primitive: CRLC_SequenceNumber_CNF begin "car_GetRLC_SeqNum" of type CRLC_SequenceNumber_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "count_C_MSB_UL" of type COUNT_C_MSB (INTEGER) [UNIVERSAL 2] matching 0 against ? end "count_C_MSB_UL" of type COUNT_C_MSB begin "count_C_LSB_UL" of type RLC_SequenceNumber (INTEGER) [UNIVERSAL 2] matching 0 against ? end "count_C_LSB_UL" of type RLC_SequenceNumber begin "count_C_MSB_DL" of type COUNT_C_MSB (INTEGER) [UNIVERSAL 2] matching 0 against ? end "count_C_MSB_DL" of type COUNT_C_MSB begin "count_C_LSB_DL" of type RLC_SequenceNumber (INTEGER) [UNIVERSAL 2] matching 0 against ? end "count_C_LSB_DL" of type RLC_SequenceNumber end "car_GetRLC_SeqNum" of type CRLC_SequenceNumber_CNF Assignment:[3] tcv_RLC_SeqNumDL_RB1 := 0 Receive event:[3] CRLC ? CRLC_SequenceNumber_CNF = PDU (view PDU) 00:01:29.600 - Primitive: CRLC_SequenceNumber_REQ Send event:[4] CRLC ! CRLC_SequenceNumber_REQ = PDU: { cellId: -1 , routingInfo: [rB_Identity: 2 ]} 00:01:29.640 - Primitive: CRLC_SequenceNumber_CNF begin "car_GetRLC_SeqNum" of type CRLC_SequenceNumber_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "count_C_MSB_UL" of type COUNT_C_MSB (INTEGER) [UNIVERSAL 2] matching 0 against ? end "count_C_MSB_UL" of type COUNT_C_MSB begin "count_C_LSB_UL" of type RLC_SequenceNumber (INTEGER) [UNIVERSAL 2] matching 2 against ? end "count_C_LSB_UL" of type RLC_SequenceNumber begin "count_C_MSB_DL" of type COUNT_C_MSB (INTEGER) [UNIVERSAL 2] matching 0 against ? end "count_C_MSB_DL" of type COUNT_C_MSB begin "count_C_LSB_DL" of type RLC_SequenceNumber (INTEGER) [UNIVERSAL 2] matching 0 against ? end "count_C_LSB_DL" of type RLC_SequenceNumber end "car_GetRLC_SeqNum" of type CRLC_SequenceNumber_CNF Assignment:[5] tcv_RLC_SeqNumDL_RB2 := 0 Receive event:[5] CRLC ? CRLC_SequenceNumber_CNF = PDU (view PDU) 00:01:29.640 - Primitive: CRLC_SequenceNumber_REQ Send event:[6] CRLC ! CRLC_SequenceNumber_REQ = PDU: { cellId: -1 , routingInfo: [rB_Identity: 3 ]} 00:01:29.680 - Primitive: CRLC_SequenceNumber_CNF begin "car_GetRLC_SeqNum" of type CRLC_SequenceNumber_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "count_C_MSB_UL" of type COUNT_C_MSB (INTEGER) [UNIVERSAL 2] matching 0 against ? end "count_C_MSB_UL" of type COUNT_C_MSB begin "count_C_LSB_UL" of type RLC_SequenceNumber (INTEGER) [UNIVERSAL 2] matching 5 against ? end "count_C_LSB_UL" of type RLC_SequenceNumber begin "count_C_MSB_DL" of type COUNT_C_MSB (INTEGER) [UNIVERSAL 2] matching 0 against ? end "count_C_MSB_DL" of type COUNT_C_MSB begin "count_C_LSB_DL" of type RLC_SequenceNumber (INTEGER) [UNIVERSAL 2] matching 3 against ? end "count_C_LSB_DL" of type RLC_SequenceNumber end "car_GetRLC_SeqNum" of type CRLC_SequenceNumber_CNF Assignment:[7] tcv_RLC_SeqNumDL_RB3 := 3 Receive event:[7] CRLC ? CRLC_SequenceNumber_CNF = PDU (view PDU) 00:01:29.680 - Primitive: CRLC_SequenceNumber_REQ Send event:[8] CRLC ! CRLC_SequenceNumber_REQ = PDU: { cellId: -1 , routingInfo: [rB_Identity: 4 ]} 00:01:29.710 - Primitive: CRLC_SequenceNumber_CNF begin "car_GetRLC_SeqNum" of type CRLC_SequenceNumber_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "count_C_MSB_UL" of type COUNT_C_MSB (INTEGER) [UNIVERSAL 2] matching 0 against ? end "count_C_MSB_UL" of type COUNT_C_MSB begin "count_C_LSB_UL" of type RLC_SequenceNumber (INTEGER) [UNIVERSAL 2] matching 0 against ? end "count_C_LSB_UL" of type RLC_SequenceNumber begin "count_C_MSB_DL" of type COUNT_C_MSB (INTEGER) [UNIVERSAL 2] matching 0 against ? end "count_C_MSB_DL" of type COUNT_C_MSB begin "count_C_LSB_DL" of type RLC_SequenceNumber (INTEGER) [UNIVERSAL 2] matching 0 against ? end "count_C_LSB_DL" of type RLC_SequenceNumber end "car_GetRLC_SeqNum" of type CRLC_SequenceNumber_CNF Assignment:[9] tcv_RLC_SeqNumDL_RB4 := 0 Receive event:[9] CRLC ? CRLC_SequenceNumber_CNF = PDU (view PDU) Attach:[17] Exit Test Step ts_CRLC_GetRLC_SeqNumSecurity
Attach:[18] Enter Test Step ts_RRC_Security::lt_AssignRB_ActivationTimeInfoList( 0 )
| Assignment:[102] tcv_RB_ActivationTimeInfoList := (view Assignment) Attach:[18] Exit Test Step ts_RRC_Security::lt_AssignRB_ActivationTimeInfoList
Attach:[19] Enter Test Step ts_CRLC_SuspendSecurity( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
00:01:29.710 - Primitive: CRLC_Suspend_REQ Send event:[2] CRLC ! CRLC_Suspend_REQ = PDU: { cellId: -1 , routingInfo: [rB_Identity: 1 ], n: 0 } 00:01:29.740 - Primitive: CRLC_Suspend_CNF begin "car_SuspendRB" of type CRLC_Suspend_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "vt" of type RLC_SequenceNumber (INTEGER) [UNIVERSAL 2] matching 0 against ? end "vt" of type RLC_SequenceNumber end "car_SuspendRB" of type CRLC_Suspend_CNF Receive event:[3] CRLC ? CRLC_Suspend_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 1 ], vt: 0 } 00:01:29.740 - Primitive: CRLC_Suspend_REQ Send event:[4] CRLC ! CRLC_Suspend_REQ = PDU: { cellId: -1 , routingInfo: [rB_Identity: 3 ], n: 3 } 00:01:29.770 - Primitive: CRLC_Suspend_CNF begin "car_SuspendRB" of type CRLC_Suspend_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "vt" of type RLC_SequenceNumber (INTEGER) [UNIVERSAL 2] matching 3 against ? end "vt" of type RLC_SequenceNumber end "car_SuspendRB" of type CRLC_Suspend_CNF Receive event:[5] CRLC ? CRLC_Suspend_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 3 ], vt: 3 } 00:01:29.770 - Primitive: CRLC_Suspend_REQ Send event:[6] CRLC ! CRLC_Suspend_REQ = PDU: { cellId: -1 , routingInfo: [rB_Identity: 4 ], n: 0 } 00:01:29.800 - Primitive: CRLC_Suspend_CNF begin "car_SuspendRB" of type CRLC_Suspend_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "vt" of type RLC_SequenceNumber (INTEGER) [UNIVERSAL 2] matching 0 against ? end "vt" of type RLC_SequenceNumber end "car_SuspendRB" of type CRLC_Suspend_CNF Receive event:[7] CRLC ? CRLC_Suspend_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 4 ], vt: 0 } Attach:[19] Exit Test Step ts_CRLC_SuspendSecurity
Attach:[20] Enter Test Step ts_CRLC_DL_CipherCfgSRB( [startRestart: uea0] )
| Attach:[1] Enter Test Step ts_CRLC_DL_CipherCfgSRB::lt_RLC_Activate( 1 )
| 00:01:29.800 - Primitive: CRLC_Ciphering_Activate_REQ Send event:[5] CRLC ! CRLC_Ciphering_Activate_REQ = PDU (view PDU) 00:01:29.820 - Primitive: CRLC_Ciphering_Activate_CNF begin "ca_CRLC_CipherActCnf" of type CRLC_Ciphering_Activate_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER end "ca_CRLC_CipherActCnf" of type CRLC_Ciphering_Activate_CNF Receive event:[6] CRLC ? CRLC_Ciphering_Activate_CNF = PDU: { cellId: -1 } Attach:[1] Exit Test Step ts_CRLC_DL_CipherCfgSRB::lt_RLC_Activate
Attach:[2] Enter Test Step ts_CRLC_DL_CipherCfgSRB::lt_RLC_Activate( 2 )
| 00:01:29.820 - Primitive: CRLC_Ciphering_Activate_REQ Send event:[5] CRLC ! CRLC_Ciphering_Activate_REQ = PDU (view PDU) 00:01:29.830 - Primitive: CRLC_Ciphering_Activate_CNF begin "ca_CRLC_CipherActCnf" of type CRLC_Ciphering_Activate_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER end "ca_CRLC_CipherActCnf" of type CRLC_Ciphering_Activate_CNF Receive event:[6] CRLC ? CRLC_Ciphering_Activate_CNF = PDU: { cellId: -1 } Attach:[2] Exit Test Step ts_CRLC_DL_CipherCfgSRB::lt_RLC_Activate
Attach:[3] Enter Test Step ts_CRLC_DL_CipherCfgSRB::lt_RLC_Activate( 3 )
| 00:01:29.830 - Primitive: CRLC_Ciphering_Activate_REQ Send event:[5] CRLC ! CRLC_Ciphering_Activate_REQ = PDU (view PDU) 00:01:29.850 - Primitive: CRLC_Ciphering_Activate_CNF begin "ca_CRLC_CipherActCnf" of type CRLC_Ciphering_Activate_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER end "ca_CRLC_CipherActCnf" of type CRLC_Ciphering_Activate_CNF Receive event:[6] CRLC ? CRLC_Ciphering_Activate_CNF = PDU: { cellId: -1 } Attach:[3] Exit Test Step ts_CRLC_DL_CipherCfgSRB::lt_RLC_Activate
Attach:[4] Enter Test Step ts_CRLC_DL_CipherCfgSRB::lt_RLC_Activate( 4 )
| 00:01:29.850 - Primitive: CRLC_Ciphering_Activate_REQ Send event:[5] CRLC ! CRLC_Ciphering_Activate_REQ = PDU (view PDU) 00:01:29.860 - Primitive: CRLC_Ciphering_Activate_CNF begin "ca_CRLC_CipherActCnf" of type CRLC_Ciphering_Activate_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER end "ca_CRLC_CipherActCnf" of type CRLC_Ciphering_Activate_CNF Receive event:[6] CRLC ? CRLC_Ciphering_Activate_CNF = PDU: { cellId: -1 } Attach:[4] Exit Test Step ts_CRLC_DL_CipherCfgSRB::lt_RLC_Activate
Attach:[20] Exit Test Step ts_CRLC_DL_CipherCfgSRB
Attach:[21] Enter Test Step ts_CRLC_DL_CipherCfgRB( [startRestart: uea0] )
| Attach:[21] Exit Test Step ts_CRLC_DL_CipherCfgRB
Attach:[22] Enter Test Step ts_CMAC_CipherCfg( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Preliminary verdict:[6] (PASS) Attach:[22] Exit Test Step ts_CMAC_CipherCfg
Attach:[4] Exit Test Step ts_RRC_Security::lt_ActivateSecurity_DL_SS
Attach:[5] Enter Test Step ts_RRC_Security::lt_RB2_UL_IntegrityActivate( 0 )
| Attach:[13] Enter Test Step ts_RB2_UL_IntegrityActivate( 0 )
| 00:01:29.860 - Primitive: CRLC_Integrity_Activate_REQ Send event:[1] CRLC ! CRLC_Integrity_Activate_REQ = PDU (view PDU) 00:01:29.880 - Primitive: CRLC_Integrity_Activate_CNF begin "ca_CRLC_IntegrityActivateCnf" of type CRLC_Integrity_Activate_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER end "ca_CRLC_IntegrityActivateCnf" of type CRLC_Integrity_Activate_CNF Receive event:[2] CRLC ? CRLC_Integrity_Activate_CNF = PDU: { cellId: -1 } Attach:[13] Exit Test Step ts_RB2_UL_IntegrityActivate
Attach:[5] Exit Test Step ts_RRC_Security::lt_RB2_UL_IntegrityActivate
Attach:[6] Enter Test Step ts_RRC_Security::lt_StartSecurity_UE( 0 )
| Attach:[27] Enter Test Step ts_RRC_Security::lt_SendSecurityModeCommand( 0 )
| 00:01:29.880 - Primitive: RLC_AM_DATA_REQ 00:01:29.880 - Primitive: RLC_AM_DATA_REQ: securityModeCommand Send event:[50] AM ! RLC_AM_DATA_REQ = PDU (view PDU) Attach:[27] Exit Test Step ts_RRC_Security::lt_SendSecurityModeCommand
00:01:30.210 - Primitive: RLC_AM_DATA_IND: securityModeComplete 00:01:30.210 - Primitive: RLC_AM_DATA_IND begin "car_RRC_SecModeCmpl" of type RLC_AM_DATA_IND (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "integrityResult" of type IntegrityResult (CHOICE) [UNIVERSAL 31] matching [integrityUsed: i_pass] against * end "integrityResult" of type IntegrityResult begin "aM_message" of type CHOICE [UNIVERSAL 31] begin "uL_DCCH_Message" of type UL_DCCH_Message (SEQUENCE) [UNIVERSAL 16] begin "integrityCheckInfo" of type IntegrityCheckInfo (SEQUENCE) [UNIVERSAL 16] matching { messageAuthenticationCode: '11000001000000010111100110000100'B , rrc_MessageSequenceNumber: 1 } against * end "integrityCheckInfo" of type IntegrityCheckInfo begin "message" of type UL_DCCH_MessageType (CHOICE) [UNIVERSAL 31] begin "securityModeComplete" of type SecurityModeComplete (SEQUENCE) [UNIVERSAL 16] begin "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier (INTEGER) [UNIVERSAL 2] matching 0 against 0 end "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier begin "ul_IntegProtActivationInfo" of type IntegrityProtActivationInfo (SEQUENCE) [UNIVERSAL 16] matching { rrc_MessageSequenceNumberList: [ 0 , 0 , 0 , 0 , 0 ] } against * end "ul_IntegProtActivationInfo" of type IntegrityProtActivationInfo begin "rb_UL_CiphActivationTimeInfo" of type RB_ActivationTimeInfoList (SEQUENCEOF) [UNIVERSAL 28] matching [ { rb_Identity: 1 , rlc_SequenceNumber: 0 } , { rb_Identity: 2 , rlc_SequenceNumber: 7 } , { rb_Identity: 3 , rlc_SequenceNumber: 5 } , { rb_Identity: 4 , rlc_SequenceNumber: 0 } ] against ? end "rb_UL_CiphActivationTimeInfo" of type RB_ActivationTimeInfoList end "securityModeComplete" of type SecurityModeComplete end "message" of type UL_DCCH_MessageType end "uL_DCCH_Message" of type UL_DCCH_Message end "aM_message" of type CHOICE end "car_RRC_SecModeCmpl" of type RLC_AM_DATA_IND Assignment:TSP1: [29] uL_Integrity := { rrc_MessageSequenceNumberList: [ 0 , 0 , 0 , 0 , 0 ] } Assignment:TSP1: [29] uL_CipherMode := (view Assignment) Receive event:TSP1: [29] AM ? RLC_AM_DATA_IND = PDU (view PDU) Preliminary verdict:TSP1: [29] (PASS) Attach:[30] Enter Test Step ts_CRLC_UL_CipherCfg( [ { rb_Identity: 1 , r ...
| (view Test Step parameters) 00:01:30.210 - Primitive: CRLC_Ciphering_Activate_REQ Send event:[1] CRLC ! CRLC_Ciphering_Activate_REQ = PDU (view PDU) 00:01:30.600 - Primitive: CRLC_Ciphering_Activate_CNF begin "ca_CRLC_CipherActCnf" of type CRLC_Ciphering_Activate_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER end "ca_CRLC_CipherActCnf" of type CRLC_Ciphering_Activate_CNF Receive event:[2] CRLC ? CRLC_Ciphering_Activate_CNF = PDU: { cellId: -1 } Attach:[30] Exit Test Step ts_CRLC_UL_CipherCfg
Attach:[31] Enter Test Step ts_CRLC_UL_Integrity( { rrc_MessageSequenceNumberList: [ 0 , 0 , 0 , 0 , 0 ] } )
| 00:01:30.600 - Primitive: CRLC_Integrity_Activate_REQ Send event:[1] CRLC ! CRLC_Integrity_Activate_REQ = PDU (view PDU) 00:01:30.610 - Primitive: CRLC_Integrity_Activate_CNF begin "ca_CRLC_IntegrityActivateCnf" of type CRLC_Integrity_Activate_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER end "ca_CRLC_IntegrityActivateCnf" of type CRLC_Integrity_Activate_CNF Receive event:[2] CRLC ? CRLC_Integrity_Activate_CNF = PDU: { cellId: -1 } Attach:[31] Exit Test Step ts_CRLC_UL_Integrity
Attach:[6] Exit Test Step ts_RRC_Security::lt_StartSecurity_UE
Attach:[8] Enter Test Step ts_CRLC_ResumeSecurity( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
00:01:30.610 - Primitive: CRLC_Resume_REQ Send event:[2] CRLC ! CRLC_Resume_REQ = PDU: { cellId: -1 , routingInfo: [rB_Identity: 1 ]} 00:01:30.640 - Primitive: CRLC_Resume_CNF begin "car_ResumeRB" of type CRLC_Resume_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "car_ResumeRB" of type CRLC_Resume_CNF Receive event:[3] CRLC ? CRLC_Resume_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 1 ]} 00:01:30.640 - Primitive: CRLC_Resume_REQ Send event:[4] CRLC ! CRLC_Resume_REQ = PDU: { cellId: -1 , routingInfo: [rB_Identity: 3 ]} 00:01:30.680 - Primitive: CRLC_Resume_CNF begin "car_ResumeRB" of type CRLC_Resume_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "car_ResumeRB" of type CRLC_Resume_CNF Receive event:[5] CRLC ? CRLC_Resume_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 3 ]} 00:01:30.680 - Primitive: CRLC_Resume_REQ Send event:[6] CRLC ! CRLC_Resume_REQ = PDU: { cellId: -1 , routingInfo: [rB_Identity: 4 ]} 00:01:30.710 - Primitive: CRLC_Resume_CNF begin "car_ResumeRB" of type CRLC_Resume_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "car_ResumeRB" of type CRLC_Resume_CNF Assignment:[7] tcv_RB_SigResumed := GcTRUE Receive event:[7] CRLC ? CRLC_Resume_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 4 ]} Attach:[8] Exit Test Step ts_CRLC_ResumeSecurity
Attach:[100] Exit Test Step ts_RRC_Security
Attach:[36] Exit Test Step ts_GMM_IdleUpdated::lt_SecurityMode
Attach:[37] Enter Test Step ts_GMM_IdleUpdated::lt_AttachAccept( 0 )
| Assignment:[102] tcv_AssignedTMSI := '11223344'O Assignment:[102] tcv_AssignedPTMSI := '12345678'O Assignment:[102] tcv_Assigned_PTMSI_Sig := 'AB1234'O 00:01:30.710 - Primitive: RRC_DATA_REQ: gmm:attachAccept 00:01:30.710 - Primitive: RLC_AM_DATA_REQ:downlinkDirectTransfer Send event:[104] Dc ! RRC_DataReq = PDU (view PDU) 00:01:31.060 - Primitive: RLC_AM_DATA_IND: uplinkDirectTransfer 00:01:31.060 - Primitive: RRC_DATA_IND: gmm:attachComplete begin "car_PS_UplinkDirectTransfer" of type RRC_DataInd (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "rB_Id" of type SS_RB_Identity (INTEGER) [UNIVERSAL 2] matching 3 against 3 end "rB_Id" of type SS_RB_Identity begin "cN_Domain" of type SS_CN_DomainIdentity (INTEGER) [UNIVERSAL 2] matching 1 against 1 end "cN_Domain" of type SS_CN_DomainIdentity begin "msg" of type ATTACHCOMPLETE (SEQUENCE) [UNIVERSAL 16] begin "skipIndicator" of type SkipIndicator (BITSTRING) [UNIVERSAL 3] matching '0000'B against '0000'B end "skipIndicator" of type SkipIndicator begin "gMMProtocolDiscriminator" of type ProtocolDiscriminator (BITSTRING) [UNIVERSAL 3] matching '1000'B against '1000'B end "gMMProtocolDiscriminator" of type ProtocolDiscriminator begin "msgType" of type MsgType (BITSTRING) [UNIVERSAL 3] matching '00000011'B against '00000011'B end "msgType" of type MsgType end "msg" of type ATTACHCOMPLETE end "car_PS_UplinkDirectTransfer" of type RRC_DataInd Receive event:[105] Dc ? RRC_DataInd = PDU (view PDU) Attach:[37] Exit Test Step ts_GMM_IdleUpdated::lt_AttachAccept
Attach:[38] Enter Test Step ts_GMM_IdleUpdated::lt_RRC_ConnRel( 0 )
| Attach:[120] Enter Test Step ts_RRC_ConnRel( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[2] Enter Test Step ts_RRC_Delay( 1000 )
| StartTimer:[1] t_Dly [5000] 1000 ms Timed out Timer:t_Dly TimeOut:[2] t_Dly [5000] 1000 ms Attach:[2] Exit Test Step ts_RRC_Delay
Attach:[3] Enter Test Step ts_RRC_ConnRel::lt_Send_RRC_ConnectionRelease( 0 )
| Assignment:[39] tcv_N308 := 1 Assignment:[39] tcv_K := 1 00:01:32.080 - Primitive: RLC_UM_DATA_REQ 00:01:32.080 - Primitive: RLC_UM_DATA_REQ: rrcConnectionRelease Send event:[40] UM ! RLC_UM_DATA_REQ = PDU (view PDU) 00:01:32.500 - Primitive: RLC_UM_DATA_IND: rrcConnectionReleaseComplete 00:01:32.500 - Primitive: RLC_UM_DATA_IND begin "car_RRC_ConnRelCmplUM" of type RLC_UM_DATA_IND (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "integrityResult" of type IntegrityResult (CHOICE) [UNIVERSAL 31] matching [integrityUsed: i_pass] against * end "integrityResult" of type IntegrityResult begin "uM_message" of type CHOICE [UNIVERSAL 31] begin "uL_DCCH_Message" of type UL_DCCH_Message (SEQUENCE) [UNIVERSAL 16] begin "integrityCheckInfo" of type IntegrityCheckInfo (SEQUENCE) [UNIVERSAL 16] matching { messageAuthenticationCode: '11110111111000101100001011001110'B , rrc_MessageSequenceNumber: 1 } against * end "integrityCheckInfo" of type IntegrityCheckInfo begin "message" of type UL_DCCH_MessageType (CHOICE) [UNIVERSAL 31] begin "rrcConnectionReleaseComplete" of type RRCConnectionReleaseComplete (SEQUENCE) [UNIVERSAL 16] begin "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier (INTEGER) [UNIVERSAL 2] matching 0 against 0 end "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier end "rrcConnectionReleaseComplete" of type RRCConnectionReleaseComplete end "message" of type UL_DCCH_MessageType end "uL_DCCH_Message" of type UL_DCCH_Message end "uM_message" of type CHOICE end "car_RRC_ConnRelCmplUM" of type RLC_UM_DATA_IND Receive event:TSP1: [41] UM ? RLC_UM_DATA_IND = PDU (view PDU) Preliminary verdict:TSP1: [41] (PASS) Attach:[42] Enter Test Step ts_RRC_ConnRel::lt_RptRcvConnRel( 0 )
| StartTimer:[49] t_Dly [5000] 5000 ms 00:01:32.640 - Primitive: RLC_UM_DATA_IND: rrcConnectionReleaseComplete 00:01:32.640 - Primitive: RLC_UM_DATA_IND begin "car_RRC_ConnRelCmplUM" of type RLC_UM_DATA_IND (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "integrityResult" of type IntegrityResult (CHOICE) [UNIVERSAL 31] matching [integrityUsed: i_pass] against * end "integrityResult" of type IntegrityResult begin "uM_message" of type CHOICE [UNIVERSAL 31] begin "uL_DCCH_Message" of type UL_DCCH_Message (SEQUENCE) [UNIVERSAL 16] begin "integrityCheckInfo" of type IntegrityCheckInfo (SEQUENCE) [UNIVERSAL 16] matching { messageAuthenticationCode: '10111001101000110000011111000000'B , rrc_MessageSequenceNumber: 2 } against * end "integrityCheckInfo" of type IntegrityCheckInfo begin "message" of type UL_DCCH_MessageType (CHOICE) [UNIVERSAL 31] begin "rrcConnectionReleaseComplete" of type RRCConnectionReleaseComplete (SEQUENCE) [UNIVERSAL 16] begin "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier (INTEGER) [UNIVERSAL 2] matching 0 against 0 end "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier end "rrcConnectionReleaseComplete" of type RRCConnectionReleaseComplete end "message" of type UL_DCCH_MessageType end "uL_DCCH_Message" of type UL_DCCH_Message end "uM_message" of type CHOICE end "car_RRC_ConnRelCmplUM" of type RLC_UM_DATA_IND Assignment:TSP2: [52] tcv_K := 2 CancelTimer:TSP2: [52] t_Dly [5000] 5000 ms Receive event:TSP2: [52] UM ? RLC_UM_DATA_IND = PDU (view PDU) Preliminary verdict:TSP2: [52] (PASS) Attach:[42] Exit Test Step ts_RRC_ConnRel::lt_RptRcvConnRel
Attach:[3] Exit Test Step ts_RRC_ConnRel::lt_Send_RRC_ConnectionRelease
Attach:[4] Enter Test Step ts_RRC_ConnRel::lt_RestartCRLC_ForNextConnection( 0 )
| Attach:[7] Enter Test Step ts_CRLC_RelReconfSRB( 0 )
| Attach:[1] Enter Test Step ts_CRLC_Rel( -1 )
| 00:01:32.640 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:32.720 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 1 ]} Attach:[1] Exit Test Step ts_CRLC_Rel
Attach:[2] Enter Test Step ts_CRLC_Rel( -1 )
| 00:01:32.720 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:32.890 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 2 ]} Attach:[2] Exit Test Step ts_CRLC_Rel
Attach:[3] Enter Test Step ts_CRLC_Rel( -1 )
| 00:01:32.890 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:32.970 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 3 ]} Attach:[3] Exit Test Step ts_CRLC_Rel
Attach:[4] Enter Test Step ts_CRLC_Rel( -1 )
| 00:01:32.970 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:33.040 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 4 ]} Attach:[4] Exit Test Step ts_CRLC_Rel
Attach:[5] Enter Test Step ts_SS_RB1_ToRB4_Cfg( )
| 00:01:33.040 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:33.180 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 1 ]} 00:01:33.180 - Primitive: CRLC_Config_REQ Send event:[3] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:33.380 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[4] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 2 ]} 00:01:33.380 - Primitive: CRLC_Config_REQ Send event:[5] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:33.520 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[6] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 3 ]} 00:01:33.520 - Primitive: CRLC_Config_REQ Send event:[7] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:33.630 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[8] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 4 ]} Attach:[5] Exit Test Step ts_SS_RB1_ToRB4_Cfg
Attach:[7] Exit Test Step ts_CRLC_RelReconfSRB
Attach:[8] Enter Test Step ts_SetCellCfg( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Assignment:[2] cellConfig := cell_DCH_StandAloneSRB_NoConn Attach:[3] Enter Test Step ts_SaveCellInfo( 0 )
| Assignment:[2] tcv_CellInfoA := (view Assignment) Attach:[3] Exit Test Step ts_SaveCellInfo
Attach:[8] Exit Test Step ts_SetCellCfg
Attach:[4] Exit Test Step ts_RRC_ConnRel::lt_RestartCRLC_ForNextConnection
Attach:[5] Enter Test Step ts_SS_ResetSecurityKey( )
| Assignment:[1] tcv_CellIndInfo := (view Assignment) Assignment:[5] cipheringAlgorithmCapability := '0000000000000001'B Attach:[5] Exit Test Step ts_SS_ResetSecurityKey
Attach:[120] Exit Test Step ts_RRC_ConnRel
Attach:[38] Exit Test Step ts_GMM_IdleUpdated::lt_RRC_ConnRel
Attach:[3] Exit Test Step ts_GMM_IdleUpdated::lt_IdleUpdated_NMO_I
Assignment:[4] tcv_Use_E_PLMN := GcFALSE Attach:[2] Exit Test Step ts_GMM_IdleUpdated
Attach:[8] Exit Test Step ts_IdleUpdated
Attach:[9] Enter Test Step ts_ToStateMO_CS_6_9_PS_6_10Or6_11( 0 )
| Attach:[1] Enter Test Step ts_AT_InitConnection( 0 )
| Attach:[1] Enter Test Step ts_AT_InitConnection::lt_UT_ConigUE_CSDomain( 0 )
| Attach:[4] Enter Test Step ts_CC_BasicServMO_Def( )
| Attach:[1] Enter Test Step ts_CC_BasicServMO( "Telephony" )
| Attach:[1] Enter Test Step ts_CC_InitTCV_MO( "Telephony" )
| Assignment:[1] tcv_ActiveService := "Telephony" Assignment:[1] tcv_CN_Domain := cs_domain Assignment:[5] tcv_CC_RB_ConfigType := cell_DCH_Speech Assignment:[5] tcv_BcapCE := '00'B Assignment:[5] tcv_EstCause := originatingConversationalCall Attach:[1] Exit Test Step ts_CC_InitTCV_MO
Attach:[2] Enter Test Step ts_UT_ConfigUE_MO( "Telephony" )
| Attach:[1] Enter Test Step ts_CC_CheckServSupported( "Telephony" )
| Assignment:[1] tcv_Res := GcFALSE Assignment:[3] tcv_Res := GcTRUE Attach:[1] Exit Test Step ts_CC_CheckServSupported
Attach:[8] Enter Test Step ts_UT_ConfigUE_MO::lt_ConfigTelephony( "Telephony" )
| 00:01:33.630 - Primitive: AT_CmdReq Send event:[19] Ut ! AT_CmdReq = PDU: { cmd: "AT+CMOD=0<CR>" , sMS_BlockMode: OMIT} 00:01:35.000 - Primitive: AT_CmdCnf begin "ca_AT_CmdCnf" of type AT_CmdCnf (SEQUENCE) [UNIVERSAL 16] begin "resultString" of type IA5String [UNIVERSAL 22] matching "<CR><LF>OK<CR><LF>" against "<CR><LF>OK<CR><LF>" IF PRESENT end "resultString" of type IA5String end "ca_AT_CmdCnf" of type AT_CmdCnf Receive event:[20] Ut ? AT_CmdCnf = PDU (view PDU) 00:01:35.000 - Primitive: MMI_CmdReq Send event:[21] Ut ! MMI_CmdReq = PDU: { cmd: "Configure UE for an MO Telephony call" } 00:01:36.050 - Primitive: MMI_CmdCnf begin "ca_MMI_CmdCnf" of type MMI_CmdCnf (SEQUENCE) [UNIVERSAL 16] begin "result" of type BOOLEAN [UNIVERSAL 1] matching GcTRUE against GcTRUE end "result" of type BOOLEAN end "ca_MMI_CmdCnf" of type MMI_CmdCnf Receive event:[22] Ut ? MMI_CmdCnf = PDU: { result: GcTRUE , resultString: OMIT} Attach:[8] Exit Test Step ts_UT_ConfigUE_MO::lt_ConfigTelephony
Attach:[2] Exit Test Step ts_UT_ConfigUE_MO
Attach:[1] Exit Test Step ts_CC_BasicServMO
Attach:[4] Exit Test Step ts_CC_BasicServMO_Def
Attach:[1] Exit Test Step ts_AT_InitConnection::lt_UT_ConigUE_CSDomain
Attach:[2] Enter Test Step ts_InitConnection( 0 )
| Attach:[2] Enter Test Step ts_AT_InitCallCS( )
| Attach:[1] Enter Test Step ts_AT_InitCallCS::lt_InitAT_Command( )
| Assignment:[5] tcv_AT_Cmd := "ATD0123456902" Assignment:[5] tcv_AT_Cmd := "ATD0123456902;" Assignment:[5] tcv_AT_Cmd := "ATD0123456902;<CR>" Attach:[1] Exit Test Step ts_AT_InitCallCS::lt_InitAT_Command
00:01:36.050 - Primitive: AT_CmdReq Send event:[2] Ut ! AT_CmdReq = PDU: { cmd: "ATD0123456902;<CR>" , sMS_BlockMode: OMIT} 00:01:37.270 - Primitive: AT_CmdCnf begin "ca_AT_CmdCnf" of type AT_CmdCnf (SEQUENCE) [UNIVERSAL 16] begin "resultString" of type IA5String [UNIVERSAL 22] matching "<CR><LF>OK<CR><LF>" against "<CR><LF>OK<CR><LF>" IF PRESENT end "resultString" of type IA5String end "ca_AT_CmdCnf" of type AT_CmdCnf Receive event:[3] Ut ? AT_CmdCnf = PDU (view PDU) Attach:[2] Exit Test Step ts_AT_InitCallCS
Attach:[2] Exit Test Step ts_InitConnection
Attach:[1] Exit Test Step ts_AT_InitConnection
Attach:[7] Enter Test Step ts_RRC_ConnEstCS_MO_P3_P4( 0 )
| Attach:[1] Enter Test Step ts_RRC_ConnEst( 0 )
| Attach:[1] Enter Test Step ts_SS_PrepareCellRRC_ConnEst( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[1] Exit Test Step ts_SS_PrepareCellRRC_ConnEst
Attach:[2] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[2] Exit Test Step ts_SetTmpCellInfo
Attach:[3] Enter Test Step ts_RRC_ConnEst::lt_RcvConnReq( 0 )
| 00:01:42.040 - Primitive: RLC_TR_DATA_IND: rrcConnectionRequest 00:01:42.040 - Primitive: RLC_TR_DATA_IND begin "car_RRC_ConnReq" of type RLC_TR_DATA_IND (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "tM_message" of type CHOICE [UNIVERSAL 31] begin "uL_CCCH_Message" of type UL_CCCH_Message (SEQUENCE) [UNIVERSAL 16] begin "message" of type UL_CCCH_MessageType (CHOICE) [UNIVERSAL 31] begin "rrcConnectionRequest" of type RRCConnectionRequest (SEQUENCE) [UNIVERSAL 16] begin "initialUE_Identity" of type InitialUE_Identity (CHOICE) [UNIVERSAL 31] begin InitialUE_Identity (CHOICE) [UNIVERSAL 31] end InitialUE_Identity begin InitialUE_Identity (CHOICE) [UNIVERSAL 31] begin "tmsi_and_LAI" of type TMSI_and_LAI_GSM_MAP (SEQUENCE) [UNIVERSAL 16] matching { tmsi: '00010001001000100011001101000100'B , lai: { plmn_Identity: { mcc: [ 0 , 0 , 1 ] , mnc: [ 0 , 1 ] } , lac: '0000000000000001'B } } against ? end "tmsi_and_LAI" of type TMSI_and_LAI_GSM_MAP end InitialUE_Identity matching [tmsi_and_LAI: { tmsi: '00010001001000100011001101000100'B , lai: { plmn_Identity: { mcc: [ 0 , 0 , 1 ] , mnc: [ 0 , 1 ] } , lac: '0000000000000001'B } } ] against ([imsi: ?], [tmsi_and_LAI: ?], [p_TMSI_and_RAI: ?], [imei: ?]) end "initialUE_Identity" of type InitialUE_Identity begin "establishmentCause" of type EstablishmentCause (ENUMERATED) [UNIVERSAL 10] matching originatingConversationalCall against originatingConversationalCall end "establishmentCause" of type EstablishmentCause begin "protocolErrorIndicator" of type ProtocolErrorIndicator (ENUMERATED) [UNIVERSAL 10] matching noError against noError end "protocolErrorIndicator" of type ProtocolErrorIndicator end "rrcConnectionRequest" of type RRCConnectionRequest end "message" of type UL_CCCH_MessageType end "uL_CCCH_Message" of type UL_CCCH_Message end "tM_message" of type CHOICE end "car_RRC_ConnReq" of type RLC_TR_DATA_IND Assignment:[9] tcv_InitialUE_Id := (view Assignment) Receive event:[9] TM ? RLC_TR_DATA_IND = PDU (view PDU) Attach:[3] Exit Test Step ts_RRC_ConnEst::lt_RcvConnReq
Attach:[4] Enter Test Step ts_RRC_ConnEst::lt_Send_ConnSetUp( 0 )
| 00:01:42.040 - Primitive: RLC_UM_DATA_REQ 00:01:42.040 - Primitive: RLC_UM_DATA_REQ: rrcConnectionSetup Send event:[31] UM ! RLC_UM_DATA_REQ = PDU (view PDU) Attach:[33] Enter Test Step ts_SetCellCfg( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Assignment:[2] cellConfig := cell_DCH_StandAloneSRB Attach:[3] Enter Test Step ts_SaveCellInfo( 0 )
| Assignment:[2] tcv_CellInfoA := (view Assignment) Attach:[3] Exit Test Step ts_SaveCellInfo
Attach:[33] Exit Test Step ts_SetCellCfg
Attach:[4] Exit Test Step ts_RRC_ConnEst::lt_Send_ConnSetUp
Attach:[5] Enter Test Step ts_RRC_ReceiveConnSetupCmpl( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
StartTimer:[3] t_WaitMS [13500] 13500 ms 00:01:42.640 - Primitive: RLC_AM_DATA_IND: rrcConnectionSetupComplete 00:01:42.660 - Primitive: RLC_AM_DATA_IND begin "car_RRC_ConnSetupCmpl" of type RLC_AM_DATA_IND (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "integrityResult" of type IntegrityResult (CHOICE) [UNIVERSAL 31] matching [integrityUsed: i_pass] against ? end "integrityResult" of type IntegrityResult begin "aM_message" of type CHOICE [UNIVERSAL 31] begin "uL_DCCH_Message" of type UL_DCCH_Message (SEQUENCE) [UNIVERSAL 16] begin "message" of type UL_DCCH_MessageType (CHOICE) [UNIVERSAL 31] begin "rrcConnectionSetupComplete" of type RRCConnectionSetupComplete (SEQUENCE) [UNIVERSAL 16] begin "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier (INTEGER) [UNIVERSAL 2] matching 0 against 0 end "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier begin "startList" of type STARTList (SEQUENCEOF) [UNIVERSAL 28] matching [ { cn_DomainIdentity: ps_domain, start_Value: '00000000000000000010'B } , { cn_DomainIdentity: cs_domain, start_Value: '00000000000000000010'B } ] against ? end "startList" of type STARTList begin "ue_RadioAccessCapability" of type UE_RadioAccessCapability (SEQUENCE) [UNIVERSAL 16] matching { accessStratumReleaseIndicator: r99, pdcp_Capability: { losslessSRNS_RelocationSupport: GcTRUE , supportForRfc2507: [supported: by8192]} , rlc_Capability: { totalRLC_AM_BufferSize: kb50, maximumRLC_WindowSize: mws2047, maximumAM_EntityNumber: am6} , transportChannelCapability: { dl_TransChCapability: { maxNoBitsReceived: b5120, maxConvCodeBitsReceived: b1280, turboDecodingSupport: [supported: b5120], maxSimultaneousTransChs: e8, maxSimultaneousCCTrCH_Count: 1 , maxReceivedTransportBlocks: tb16, maxNumberOfTFC: tfc96, maxNumberOfTF: tf64} , ul_TransChCapability: { maxNoBitsTransmitted: b3840, maxConvCodeBitsTransmitted: b1280, turboEncodingSupport: [supported: b3840], maxSimultaneousTransChs: e8, modeSpecificInfo: [fdd: NULL], maxTransmittedBlocks: tb8, maxNumberOfTFC: tfc32, maxNumberOfTF: tf32} } , rf_Capability: { fddRF_Capability: { ue_PowerClass: 4 , txRxFrequencySeparation: mhz190} , tddRF_Capability: OMIT} , physicalChannelCapability: { fddPhysChCapability: { downlinkPhysChCapability: { maxNoDPCH_PDSCH_Codes: 3 , maxNoPhysChBitsReceived: b9600, supportForSF_512: GcFALSE , supportOfPDSCH: GcFALSE , simultaneousSCCPCH_DPCH_Reception: [notSupported: NULL]} , uplinkPhysChCapability: { maxNoDPDCH_BitsTransmitted: b2400, supportOfPCPCH: GcFALSE } } , tddPhysChCapability: OMIT} , ue_MultiModeRAT_Capability: { multiRAT_CapabilityList: { supportOfGSM: GcFALSE , supportOfMulticarrier: GcFALSE } , multiModeCapability: fdd} , securityCapability: { cipheringAlgorithmCap: '0000000000000001'B , integrityProtectionAlgorithmCap: '0000000000000010'B } , ue_positioning_Capability: { standaloneLocMethodsSupported: GcFALSE , ue_BasedOTDOA_Supported: GcFALSE , networkAssistedGPS_Supported: noNetworkAssistedGPS, supportForUE_GPS_TimingOfCellFrames: GcFALSE , supportForIPDL: GcFALSE } , measurementCapability: { downlinkCompressedMode: { fdd_Measurements: GcTRUE , tdd_Measurements: OMIT, gsm_Measurements: { gsm900: GcTRUE , dcs1800: GcTRUE , gsm1900: GcFALSE } , multiCarrierMeasurements: GcFALSE } , uplinkCompressedMode: { fdd_Measurements: GcTRUE , tdd_Measurements: OMIT, gsm_Measurements: { gsm900: GcTRUE , dcs1800: GcTRUE , gsm1900: GcFALSE } , multiCarrierMeasurements: GcFALSE } } } against * end "ue_RadioAccessCapability" of type UE_RadioAccessCapability end "rrcConnectionSetupComplete" of type RRCConnectionSetupComplete end "message" of type UL_DCCH_MessageType end "uL_DCCH_Message" of type UL_DCCH_Message end "aM_message" of type CHOICE end "car_RRC_ConnSetupCmpl" of type RLC_AM_DATA_IND Assignment:TSP1: [5] tcv_StartList := (view Assignment) Assignment:TSP1: [5] cipheringAlgorithmCapability := '0000000000000001'B CancelTimer:TSP1: [5] t_WaitMS [13500] 13500 ms Receive event:TSP1: [5] AM ? RLC_AM_DATA_IND = PDU (view PDU) Preliminary verdict:TSP1: [5] (PASS) Attach:[6] Enter Test Step ts_RRC_ReceiveConnSetupCmpl::lt_GetHFN( 0 )
| Assignment:[13] tcv_Count := 2 Attach:[17] Enter Test Step ts_RRC_ReceiveConnSetupCmpl::lt_FirstValue( 0 )
| Assignment:[23] start_PS := '00000000000000000010'B Attach:[17] Exit Test Step ts_RRC_ReceiveConnSetupCmpl::lt_FirstValue
Attach:[18] Enter Test Step ts_RRC_ReceiveConnSetupCmpl::lt_SecondValue( 0 )
| Assignment:[26] start_CS := '00000000000000000010'B Attach:[18] Exit Test Step ts_RRC_ReceiveConnSetupCmpl::lt_SecondValue
Attach:[6] Exit Test Step ts_RRC_ReceiveConnSetupCmpl::lt_GetHFN
Attach:[5] Exit Test Step ts_RRC_ReceiveConnSetupCmpl
Attach:[1] Exit Test Step ts_RRC_ConnEst
Attach:[2] Enter Test Step ts_MM_CM_ServReqDef( 0 )
| Attach:[2] Exit Test Step ts_MM_CM_ServReqDef
00:01:42.660 - Primitive: RLC_AM_DATA_IND: initialDirectTransfer 00:01:42.660 - Primitive: RRC_DATA_IND: mm:cmServiceRequest Attach:[2] Enter Test Step ts_MM_CM_ServReqDef( 0 )
| begin "car_InitDirectTransfer" of type RRC_DataInd (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "rB_Id" of type SS_RB_Identity (INTEGER) [UNIVERSAL 2] matching 3 against 3 end "rB_Id" of type SS_RB_Identity begin "cN_Domain" of type SS_CN_DomainIdentity (INTEGER) [UNIVERSAL 2] matching 0 against 0 end "cN_Domain" of type SS_CN_DomainIdentity begin "start" of type START_Value (BITSTRING) [UNIVERSAL 3] matching '00000000000000000010'B against ? end "start" of type START_Value begin "msg" of type CMSERVICEREQUEST (SEQUENCE) [UNIVERSAL 16] begin "skipIndicator" of type SkipIndicator (BITSTRING) [UNIVERSAL 3] matching '0000'B against '0000'B end "skipIndicator" of type SkipIndicator begin "mMProtocolDiscriminator" of type ProtocolDiscriminator (BITSTRING) [UNIVERSAL 3] matching '0101'B against '0101'B end "mMProtocolDiscriminator" of type ProtocolDiscriminator begin "msgType" of type MsgType (BITSTRING) [UNIVERSAL 3] matching '00100100'B against '??100100'B end "msgType" of type MsgType begin "ciphKeySeqNum" of type CiphKeySeqNum (SEQUENCE) [UNIVERSAL 16] begin "spare1" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against '0'B end "spare1" of type B1 begin "keySeq" of type KeySeq (BITSTRING) [UNIVERSAL 3] matching '000'B against ? end "keySeq" of type KeySeq end "ciphKeySeqNum" of type CiphKeySeqNum begin "cMServType" of type CMServType (BITSTRING) [UNIVERSAL 3] matching '0001'B against ? end "cMServType" of type CMServType begin "mSClsmk2" of type MS_Clsmk2_lv (SEQUENCE) [UNIVERSAL 16] begin "iel" of type Length (OCTETSTRING) [UNIVERSAL 4] matching '03'O against '03'O end "iel" of type Length begin "spare1_1" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against '0'B end "spare1_1" of type B1 begin "revLvl" of type B2 (BITSTRING) [UNIVERSAL 3] matching '10'B against ? end "revLvl" of type B2 begin "eSIND" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against ? end "eSIND" of type B1 begin "a5_1" of type B1 (BITSTRING) [UNIVERSAL 3] matching '1'B against ? end "a5_1" of type B1 begin "rFPwrCap" of type B3 (BITSTRING) [UNIVERSAL 3] matching '111'B against ? end "rFPwrCap" of type B3 begin "spare1_2" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against '0'B end "spare1_2" of type B1 begin "pSCap" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against ? end "pSCap" of type B1 begin "sSSI" of type B2 (BITSTRING) [UNIVERSAL 3] matching '01'B against ? end "sSSI" of type B2 begin "sMCap" of type B1 (BITSTRING) [UNIVERSAL 3] matching '1'B against ? end "sMCap" of type B1 begin "vBS" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against ? end "vBS" of type B1 begin "vGCS" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against ? end "vGCS" of type B1 begin "fC" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against ? end "fC" of type B1 begin "cM3" of type B1 (BITSTRING) [UNIVERSAL 3] matching '1'B against ? end "cM3" of type B1 begin "spare1_3" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against '0'B end "spare1_3" of type B1 begin "lCSVA" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against ? end "lCSVA" of type B1 begin "uCS2" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against ? end "uCS2" of type B1 begin "soLSA" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against ? end "soLSA" of type B1 begin "cMSP" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against ? end "cMSP" of type B1 begin "a5_3" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against ? end "a5_3" of type B1 begin "a5_2" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against ? end "a5_2" of type B1 end "mSClsmk2" of type MS_Clsmk2_lv begin "mobileId" of type MS_Identity_lv (SEQUENCE) [UNIVERSAL 16] begin "iel" of type Length (OCTETSTRING) [UNIVERSAL 4] matching '05'O against ? end "iel" of type Length begin "iDigit1" of type B4 (BITSTRING) [UNIVERSAL 3] matching '1111'B against ? end "iDigit1" of type B4 begin "oddEvenInd" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against ? end "oddEvenInd" of type B1 begin "typeOfId" of type B3 (BITSTRING) [UNIVERSAL 3] matching '100'B against ? end "typeOfId" of type B3 begin "otherDigits" of type OCTETSTRING [UNIVERSAL 4] matching '11223344'O against ? end "otherDigits" of type OCTETSTRING end "mobileId" of type MS_Identity_lv end "msg" of type CMSERVICEREQUEST end "car_InitDirectTransfer" of type RRC_DataInd Assignment:[1] tcv_Start := '00000000000000000010'B Receive event:[1] Dc ? RRC_DataInd = PDU (view PDU) Attach:[2] Enter Test Step ts_SS_SecurityDownloadStart( cs_domain )
| Assignment:[2] start_CS := '00000000000000000010'B Attach:[2] Exit Test Step ts_SS_SecurityDownloadStart
Attach:[2] Exit Test Step ts_MM_CM_ServReqDef
Attach:[7] Exit Test Step ts_RRC_ConnEstCS_MO_P3_P4
Attach:[8] Enter Test Step ts_RRC_NAS_CallSetupCS_MO_P7_P8( 0 )
| Attach:[1] Enter Test Step ts_MM_Authentication( 0 )
| Attach:[1] Enter Test Step ts_MM_AuthenticationInit( )
| Attach:[1] Enter Test Step ts_MM_AuthenticationInit::lt_IncrementCiphKeySeqNum( )
| Assignment:[6] tcv_CS_KeySeq := '001'B Attach:[1] Exit Test Step ts_MM_AuthenticationInit::lt_IncrementCiphKeySeqNum
Attach:[2] Enter Test Step ts_MM_AuthenticationInit::lt_AuthCalcAUTN( )
| Assignment:[19] tcv_AuthXDOUT := (view Assignment) Assignment:[20] tcv_AuthCDOUT := '0000000000000000000000000000000000000000000000000000000000000000'B Assignment:[21] tcv_AuthXDOUT_Half := '0101010101000100011101110110011000010001000000000011001100100010'B Assignment:[22] tcv_AuthAK := '011001100001000100000000001100110010001011011101'B Assignment:[23] tcv_AuthAUTN_1 := '011001100001000100000000001100110010001011011101'B Assignment:[24] tcv_AuthMAC := '0101010101000100011101110110011000010001000000000011001100100010'B Assignment:[25] tcv_AuthAUTN_2 := (view Assignment) Assignment:[26] tcv_AuthAUTN := (view Assignment) Attach:[2] Exit Test Step ts_MM_AuthenticationInit::lt_AuthCalcAUTN
Attach:[3] Enter Test Step ts_MM_AuthenticationInit::lt_AuthCalcUMTS_Others( )
| Assignment:[27] tcv_AuthIK := (view Assignment) Assignment:[28] tcv_AuthCK := (view Assignment) Assignment:[29] tcv_AuthXRES := (view Assignment) Attach:[3] Exit Test Step ts_MM_AuthenticationInit::lt_AuthCalcUMTS_Others
Attach:[4] Enter Test Step ts_MM_AuthenticationInit::lt_AuthCalcKcGSM( )
| Assignment:[30] tcv_AuthCK_1 := '0100010001110111011001100001000100000000001100110010001011011101'B Assignment:[31] tcv_AuthCK_2 := '1100110011111111111011101001100110001000101110111010101001010101'B Assignment:[32] tcv_AuthIK_1 := '0111011101100110000100010000000000110011001000101101110111001100'B Assignment:[33] tcv_AuthIK_2 := '1111111111101110100110011000100010111011101010100101010101000100'B Assignment:[34] tcv_AuthCK_XOR := '1000100010001000100010001000100010001000100010001000100010001000'B Assignment:[35] tcv_AuthIK_XOR := '1000100010001000100010001000100010001000100010001000100010001000'B Assignment:[36] tcv_AuthKcGSM := '0000000000000000000000000000000000000000000000000000000000000000'B Attach:[4] Exit Test Step ts_MM_AuthenticationInit::lt_AuthCalcKcGSM
Attach:[1] Exit Test Step ts_MM_AuthenticationInit
00:01:42.680 - Primitive: RRC_DATA_REQ: mm:authenticationRequest 00:01:42.690 - Primitive: RLC_AM_DATA_REQ:downlinkDirectTransfer Send event:[2] Dc ! RRC_DataReq = PDU (view PDU) 00:01:43.130 - Primitive: RLC_AM_DATA_IND: uplinkDirectTransfer 00:01:43.130 - Primitive: RRC_DATA_IND: mm:authenticationResponse begin "car_UplinkDirectTransfer" of type RRC_DataInd (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "rB_Id" of type SS_RB_Identity (INTEGER) [UNIVERSAL 2] matching 3 against 3 end "rB_Id" of type SS_RB_Identity begin "cN_Domain" of type SS_CN_DomainIdentity (INTEGER) [UNIVERSAL 2] matching 0 against 0 end "cN_Domain" of type SS_CN_DomainIdentity begin "msg" of type AUTHENTICATIONRESPONSE (SEQUENCE) [UNIVERSAL 16] begin "skipIndicator" of type SkipIndicator (BITSTRING) [UNIVERSAL 3] matching '0000'B against '0000'B end "skipIndicator" of type SkipIndicator begin "mMProtocolDiscriminator" of type ProtocolDiscriminator (BITSTRING) [UNIVERSAL 3] matching '0101'B against '0101'B end "mMProtocolDiscriminator" of type ProtocolDiscriminator begin "msgType" of type MsgType (BITSTRING) [UNIVERSAL 3] matching '01010100'B against '??010100'B end "msgType" of type MsgType begin "authRsp" of type AuthRsp (BITSTRING) [UNIVERSAL 3] matching '01010101010001000111011101100110'B against ? end "authRsp" of type AuthRsp begin "authRspExt" of type AuthRspExt (SEQUENCE) [UNIVERSAL 16] begin "iei" of type IEI8 (BITSTRING) [UNIVERSAL 3] matching '00100001'B against '00100001'B end "iei" of type IEI8 begin "iel" of type Length (OCTETSTRING) [UNIVERSAL 4] matching '0C'O against ? end "iel" of type Length begin "rES" of type BITSTRING [UNIVERSAL 3] matching '000100010000000000110011001000101101110111001100111111111110111010011001100010001011101110101010'B against ? end "rES" of type BITSTRING end "authRspExt" of type AuthRspExt end "msg" of type AUTHENTICATIONRESPONSE end "car_UplinkDirectTransfer" of type RRC_DataInd Assignment:[3] tcv_AuthRspPDU (view PDU) Assignment:[3] tcv_AuthRsp := '01010101010001000111011101100110'B Assignment:[3] tcv_AuthRspExt := (view Assignment) Receive event:[3] Dc ? RRC_DataInd = PDU (view PDU) Assignment:[4] tcv_Res := GcTRUE Attach:[1] Exit Test Step ts_MM_Authentication
Attach:[2] Enter Test Step ts_RRC_Security( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[2] Enter Test Step ts_RRC_Security::lt_RRC_InitVariables( 0 )
| Attach:[53] Enter Test Step ts_RRC_Security::lt_InitCipherMode( 0 )
| Assignment:[76] dL_CipherMode := [startRestart: uea0] Assignment:[76] cipheringAlgorithmCapability := '0000000000000001'B Assignment:[78] cs_cipheringStarted := GcTRUE Attach:[53] Exit Test Step ts_RRC_Security::lt_InitCipherMode
Attach:[54] Enter Test Step ts_RRC_Security::lt_InitIntegrity( 0 )
| Assignment:[87] recentSecureDomain := cs_domain Assignment:[92] dL_Integrity := (view Assignment) Assignment:[92] integrityStarted := GcTRUE Assignment:[92] dl_IntegrityCheckInfo := (view Assignment) Assignment:[92] tcv_Int_ModifyFlag := GcFALSE Attach:[54] Exit Test Step ts_RRC_Security::lt_InitIntegrity
Attach:[55] Enter Test Step ts_InitSystemSpecificCap( )
| Assignment:[11] tcv_UE_SystemSpecificCap := 0 Attach:[55] Exit Test Step ts_InitSystemSpecificCap
Attach:[56] Enter Test Step ts_SaveCellInfo( 0 )
| Assignment:[2] tcv_CellInfoA := (view Assignment) Attach:[56] Exit Test Step ts_SaveCellInfo
Assignment:[58] tcv_HFN := '00000000000000000000'B Assignment:[60] start_CS := '00000000000000000000'B Attach:[2] Exit Test Step ts_RRC_Security::lt_RRC_InitVariables
Attach:[3] Enter Test Step ts_SS_DownloadSecurityKey( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[6] Enter Test Step ts_SS_DownloadSecurityKey::lt_DownloadKeyCRLC( '00000000000000000000'B )
| 00:01:43.140 - Primitive: CRLC_SecurityMode_Config_REQ 00:01:43.140 - Primitive: CRLC_SecurityMode_Config_REQ Send event:[21] CRLC ! CRLC_SecurityMode_Config_REQ = PDU (view PDU) 00:01:43.160 - Primitive: CRLC_SecurityMode_Config_CNF begin "ca_CRLC_SecurityModeCfgCnf" of type CRLC_SecurityMode_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER end "ca_CRLC_SecurityModeCfgCnf" of type CRLC_SecurityMode_Config_CNF Receive event:[22] CRLC ? CRLC_SecurityMode_Config_CNF = PDU: { cellId: -1 } Attach:[6] Exit Test Step ts_SS_DownloadSecurityKey::lt_DownloadKeyCRLC
Attach:[3] Exit Test Step ts_SS_DownloadSecurityKey
Attach:[4] Enter Test Step ts_RRC_Security::lt_ActivateSecurity_DL_SS( 0 )
| Attach:[14] Enter Test Step ts_RRC_Security::lt_InitialiseRRC_MSN( 0 )
| Attach:[25] Enter Test Step ts_SetDL_RRC_MessageSN( 0 )
| 00:01:43.160 - Primitive: CRLC_SetRRC_MessageSN_REQ Send event:[1] CRLC ! CRLC_SetRRC_MessageSN_REQ = PDU (view PDU) 00:01:43.180 - Primitive: CRLC_SetRRC_MessageSN_CNF begin "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF Receive event:[2] CRLC ? CRLC_SetRRC_MessageSN_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: 0 ]} 00:01:43.180 - Primitive: CRLC_SetRRC_MessageSN_REQ Send event:[3] CRLC ! CRLC_SetRRC_MessageSN_REQ = PDU (view PDU) 00:01:43.190 - Primitive: CRLC_SetRRC_MessageSN_CNF begin "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF Receive event:[4] CRLC ? CRLC_SetRRC_MessageSN_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 1 ]} 00:01:43.190 - Primitive: CRLC_SetRRC_MessageSN_REQ Send event:[5] CRLC ! CRLC_SetRRC_MessageSN_REQ = PDU (view PDU) 00:01:43.210 - Primitive: CRLC_SetRRC_MessageSN_CNF begin "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF Receive event:[6] CRLC ? CRLC_SetRRC_MessageSN_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 2 ]} 00:01:43.210 - Primitive: CRLC_SetRRC_MessageSN_REQ Send event:[7] CRLC ! CRLC_SetRRC_MessageSN_REQ = PDU (view PDU) 00:01:43.220 - Primitive: CRLC_SetRRC_MessageSN_CNF begin "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF Receive event:[8] CRLC ? CRLC_SetRRC_MessageSN_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 3 ]} 00:01:43.220 - Primitive: CRLC_SetRRC_MessageSN_REQ Send event:[9] CRLC ! CRLC_SetRRC_MessageSN_REQ = PDU (view PDU) 00:01:43.240 - Primitive: CRLC_SetRRC_MessageSN_CNF begin "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_SetRRC_MSN_CNF" of type CRLC_SetRRC_MessageSN_CNF Receive event:[10] CRLC ? CRLC_SetRRC_MessageSN_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 4 ]} Attach:[25] Exit Test Step ts_SetDL_RRC_MessageSN
Attach:[14] Exit Test Step ts_RRC_Security::lt_InitialiseRRC_MSN
Attach:[15] Enter Test Step ts_CRLC_DL_Integrity( { integrityProtectionM ...
| (view Test Step parameters) 00:01:43.240 - Primitive: CRLC_Integrity_Activate_REQ 00:01:43.240 - Primitive: CRLC_Integrity_Activate_REQ Send event:[1] CRLC ! CRLC_Integrity_Activate_REQ = PDU (view PDU) 00:01:43.250 - Primitive: CRLC_Integrity_Activate_CNF begin "ca_CRLC_IntegrityActivateCnf" of type CRLC_Integrity_Activate_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER end "ca_CRLC_IntegrityActivateCnf" of type CRLC_Integrity_Activate_CNF Receive event:[2] CRLC ? CRLC_Integrity_Activate_CNF = PDU: { cellId: -1 } Attach:[15] Exit Test Step ts_CRLC_DL_Integrity
Attach:[17] Enter Test Step ts_CRLC_GetRLC_SeqNumSecurity( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
00:01:43.250 - Primitive: CRLC_SequenceNumber_REQ Send event:[2] CRLC ! CRLC_SequenceNumber_REQ = PDU: { cellId: -1 , routingInfo: [rB_Identity: 1 ]} 00:01:43.290 - Primitive: CRLC_SequenceNumber_CNF begin "car_GetRLC_SeqNum" of type CRLC_SequenceNumber_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "count_C_MSB_UL" of type COUNT_C_MSB (INTEGER) [UNIVERSAL 2] matching 0 against ? end "count_C_MSB_UL" of type COUNT_C_MSB begin "count_C_LSB_UL" of type RLC_SequenceNumber (INTEGER) [UNIVERSAL 2] matching 0 against ? end "count_C_LSB_UL" of type RLC_SequenceNumber begin "count_C_MSB_DL" of type COUNT_C_MSB (INTEGER) [UNIVERSAL 2] matching 0 against ? end "count_C_MSB_DL" of type COUNT_C_MSB begin "count_C_LSB_DL" of type RLC_SequenceNumber (INTEGER) [UNIVERSAL 2] matching 0 against ? end "count_C_LSB_DL" of type RLC_SequenceNumber end "car_GetRLC_SeqNum" of type CRLC_SequenceNumber_CNF Assignment:[3] tcv_RLC_SeqNumDL_RB1 := 0 Receive event:[3] CRLC ? CRLC_SequenceNumber_CNF = PDU (view PDU) 00:01:43.290 - Primitive: CRLC_SequenceNumber_REQ Send event:[4] CRLC ! CRLC_SequenceNumber_REQ = PDU: { cellId: -1 , routingInfo: [rB_Identity: 2 ]} 00:01:43.320 - Primitive: CRLC_SequenceNumber_CNF begin "car_GetRLC_SeqNum" of type CRLC_SequenceNumber_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "count_C_MSB_UL" of type COUNT_C_MSB (INTEGER) [UNIVERSAL 2] matching 0 against ? end "count_C_MSB_UL" of type COUNT_C_MSB begin "count_C_LSB_UL" of type RLC_SequenceNumber (INTEGER) [UNIVERSAL 2] matching 2 against ? end "count_C_LSB_UL" of type RLC_SequenceNumber begin "count_C_MSB_DL" of type COUNT_C_MSB (INTEGER) [UNIVERSAL 2] matching 0 against ? end "count_C_MSB_DL" of type COUNT_C_MSB begin "count_C_LSB_DL" of type RLC_SequenceNumber (INTEGER) [UNIVERSAL 2] matching 0 against ? end "count_C_LSB_DL" of type RLC_SequenceNumber end "car_GetRLC_SeqNum" of type CRLC_SequenceNumber_CNF Assignment:[5] tcv_RLC_SeqNumDL_RB2 := 0 Receive event:[5] CRLC ? CRLC_SequenceNumber_CNF = PDU (view PDU) 00:01:43.320 - Primitive: CRLC_SequenceNumber_REQ Send event:[6] CRLC ! CRLC_SequenceNumber_REQ = PDU: { cellId: -1 , routingInfo: [rB_Identity: 3 ]} 00:01:43.350 - Primitive: CRLC_SequenceNumber_CNF begin "car_GetRLC_SeqNum" of type CRLC_SequenceNumber_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "count_C_MSB_UL" of type COUNT_C_MSB (INTEGER) [UNIVERSAL 2] matching 0 against ? end "count_C_MSB_UL" of type COUNT_C_MSB begin "count_C_LSB_UL" of type RLC_SequenceNumber (INTEGER) [UNIVERSAL 2] matching 4 against ? end "count_C_LSB_UL" of type RLC_SequenceNumber begin "count_C_MSB_DL" of type COUNT_C_MSB (INTEGER) [UNIVERSAL 2] matching 0 against ? end "count_C_MSB_DL" of type COUNT_C_MSB begin "count_C_LSB_DL" of type RLC_SequenceNumber (INTEGER) [UNIVERSAL 2] matching 3 against ? end "count_C_LSB_DL" of type RLC_SequenceNumber end "car_GetRLC_SeqNum" of type CRLC_SequenceNumber_CNF Assignment:[7] tcv_RLC_SeqNumDL_RB3 := 3 Receive event:[7] CRLC ? CRLC_SequenceNumber_CNF = PDU (view PDU) 00:01:43.350 - Primitive: CRLC_SequenceNumber_REQ Send event:[8] CRLC ! CRLC_SequenceNumber_REQ = PDU: { cellId: -1 , routingInfo: [rB_Identity: 4 ]} 00:01:43.390 - Primitive: CRLC_SequenceNumber_CNF begin "car_GetRLC_SeqNum" of type CRLC_SequenceNumber_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "count_C_MSB_UL" of type COUNT_C_MSB (INTEGER) [UNIVERSAL 2] matching 0 against ? end "count_C_MSB_UL" of type COUNT_C_MSB begin "count_C_LSB_UL" of type RLC_SequenceNumber (INTEGER) [UNIVERSAL 2] matching 0 against ? end "count_C_LSB_UL" of type RLC_SequenceNumber begin "count_C_MSB_DL" of type COUNT_C_MSB (INTEGER) [UNIVERSAL 2] matching 0 against ? end "count_C_MSB_DL" of type COUNT_C_MSB begin "count_C_LSB_DL" of type RLC_SequenceNumber (INTEGER) [UNIVERSAL 2] matching 0 against ? end "count_C_LSB_DL" of type RLC_SequenceNumber end "car_GetRLC_SeqNum" of type CRLC_SequenceNumber_CNF Assignment:[9] tcv_RLC_SeqNumDL_RB4 := 0 Receive event:[9] CRLC ? CRLC_SequenceNumber_CNF = PDU (view PDU) Attach:[17] Exit Test Step ts_CRLC_GetRLC_SeqNumSecurity
Attach:[18] Enter Test Step ts_RRC_Security::lt_AssignRB_ActivationTimeInfoList( 0 )
| Assignment:[102] tcv_RB_ActivationTimeInfoList := (view Assignment) Attach:[18] Exit Test Step ts_RRC_Security::lt_AssignRB_ActivationTimeInfoList
Attach:[19] Enter Test Step ts_CRLC_SuspendSecurity( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
00:01:43.390 - Primitive: CRLC_Suspend_REQ Send event:[2] CRLC ! CRLC_Suspend_REQ = PDU: { cellId: -1 , routingInfo: [rB_Identity: 1 ], n: 0 } 00:01:43.430 - Primitive: CRLC_Suspend_CNF begin "car_SuspendRB" of type CRLC_Suspend_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "vt" of type RLC_SequenceNumber (INTEGER) [UNIVERSAL 2] matching 0 against ? end "vt" of type RLC_SequenceNumber end "car_SuspendRB" of type CRLC_Suspend_CNF Receive event:[3] CRLC ? CRLC_Suspend_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 1 ], vt: 0 } 00:01:43.430 - Primitive: CRLC_Suspend_REQ Send event:[4] CRLC ! CRLC_Suspend_REQ = PDU: { cellId: -1 , routingInfo: [rB_Identity: 3 ], n: 3 } 00:01:43.460 - Primitive: CRLC_Suspend_CNF begin "car_SuspendRB" of type CRLC_Suspend_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "vt" of type RLC_SequenceNumber (INTEGER) [UNIVERSAL 2] matching 3 against ? end "vt" of type RLC_SequenceNumber end "car_SuspendRB" of type CRLC_Suspend_CNF Receive event:[5] CRLC ? CRLC_Suspend_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 3 ], vt: 3 } 00:01:43.460 - Primitive: CRLC_Suspend_REQ Send event:[6] CRLC ! CRLC_Suspend_REQ = PDU: { cellId: -1 , routingInfo: [rB_Identity: 4 ], n: 0 } 00:01:43.490 - Primitive: CRLC_Suspend_CNF begin "car_SuspendRB" of type CRLC_Suspend_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "vt" of type RLC_SequenceNumber (INTEGER) [UNIVERSAL 2] matching 0 against ? end "vt" of type RLC_SequenceNumber end "car_SuspendRB" of type CRLC_Suspend_CNF Receive event:[7] CRLC ? CRLC_Suspend_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 4 ], vt: 0 } Attach:[19] Exit Test Step ts_CRLC_SuspendSecurity
Attach:[20] Enter Test Step ts_CRLC_DL_CipherCfgSRB( [startRestart: uea0] )
| Attach:[1] Enter Test Step ts_CRLC_DL_CipherCfgSRB::lt_RLC_Activate( 1 )
| 00:01:43.490 - Primitive: CRLC_Ciphering_Activate_REQ Send event:[5] CRLC ! CRLC_Ciphering_Activate_REQ = PDU (view PDU) 00:01:43.500 - Primitive: CRLC_Ciphering_Activate_CNF begin "ca_CRLC_CipherActCnf" of type CRLC_Ciphering_Activate_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER end "ca_CRLC_CipherActCnf" of type CRLC_Ciphering_Activate_CNF Receive event:[6] CRLC ? CRLC_Ciphering_Activate_CNF = PDU: { cellId: -1 } Attach:[1] Exit Test Step ts_CRLC_DL_CipherCfgSRB::lt_RLC_Activate
Attach:[2] Enter Test Step ts_CRLC_DL_CipherCfgSRB::lt_RLC_Activate( 2 )
| 00:01:43.500 - Primitive: CRLC_Ciphering_Activate_REQ Send event:[5] CRLC ! CRLC_Ciphering_Activate_REQ = PDU (view PDU) 00:01:43.520 - Primitive: CRLC_Ciphering_Activate_CNF begin "ca_CRLC_CipherActCnf" of type CRLC_Ciphering_Activate_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER end "ca_CRLC_CipherActCnf" of type CRLC_Ciphering_Activate_CNF Receive event:[6] CRLC ? CRLC_Ciphering_Activate_CNF = PDU: { cellId: -1 } Attach:[2] Exit Test Step ts_CRLC_DL_CipherCfgSRB::lt_RLC_Activate
Attach:[3] Enter Test Step ts_CRLC_DL_CipherCfgSRB::lt_RLC_Activate( 3 )
| 00:01:43.520 - Primitive: CRLC_Ciphering_Activate_REQ Send event:[5] CRLC ! CRLC_Ciphering_Activate_REQ = PDU (view PDU) 00:01:43.540 - Primitive: CRLC_Ciphering_Activate_CNF begin "ca_CRLC_CipherActCnf" of type CRLC_Ciphering_Activate_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER end "ca_CRLC_CipherActCnf" of type CRLC_Ciphering_Activate_CNF Receive event:[6] CRLC ? CRLC_Ciphering_Activate_CNF = PDU: { cellId: -1 } Attach:[3] Exit Test Step ts_CRLC_DL_CipherCfgSRB::lt_RLC_Activate
Attach:[4] Enter Test Step ts_CRLC_DL_CipherCfgSRB::lt_RLC_Activate( 4 )
| 00:01:43.540 - Primitive: CRLC_Ciphering_Activate_REQ Send event:[5] CRLC ! CRLC_Ciphering_Activate_REQ = PDU (view PDU) 00:01:43.550 - Primitive: CRLC_Ciphering_Activate_CNF begin "ca_CRLC_CipherActCnf" of type CRLC_Ciphering_Activate_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER end "ca_CRLC_CipherActCnf" of type CRLC_Ciphering_Activate_CNF Receive event:[6] CRLC ? CRLC_Ciphering_Activate_CNF = PDU: { cellId: -1 } Attach:[4] Exit Test Step ts_CRLC_DL_CipherCfgSRB::lt_RLC_Activate
Attach:[20] Exit Test Step ts_CRLC_DL_CipherCfgSRB
Attach:[21] Enter Test Step ts_CRLC_DL_CipherCfgRB( [startRestart: uea0] )
| Attach:[21] Exit Test Step ts_CRLC_DL_CipherCfgRB
Attach:[22] Enter Test Step ts_CMAC_CipherCfg( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Preliminary verdict:[6] (PASS) Attach:[22] Exit Test Step ts_CMAC_CipherCfg
Attach:[4] Exit Test Step ts_RRC_Security::lt_ActivateSecurity_DL_SS
Attach:[5] Enter Test Step ts_RRC_Security::lt_RB2_UL_IntegrityActivate( 0 )
| Attach:[13] Enter Test Step ts_RB2_UL_IntegrityActivate( 0 )
| 00:01:43.550 - Primitive: CRLC_Integrity_Activate_REQ Send event:[1] CRLC ! CRLC_Integrity_Activate_REQ = PDU (view PDU) 00:01:43.570 - Primitive: CRLC_Integrity_Activate_CNF begin "ca_CRLC_IntegrityActivateCnf" of type CRLC_Integrity_Activate_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER end "ca_CRLC_IntegrityActivateCnf" of type CRLC_Integrity_Activate_CNF Receive event:[2] CRLC ? CRLC_Integrity_Activate_CNF = PDU: { cellId: -1 } Attach:[13] Exit Test Step ts_RB2_UL_IntegrityActivate
Attach:[5] Exit Test Step ts_RRC_Security::lt_RB2_UL_IntegrityActivate
Attach:[6] Enter Test Step ts_RRC_Security::lt_StartSecurity_UE( 0 )
| Attach:[27] Enter Test Step ts_RRC_Security::lt_SendSecurityModeCommand( 0 )
| 00:01:43.570 - Primitive: RLC_AM_DATA_REQ 00:01:43.570 - Primitive: RLC_AM_DATA_REQ: securityModeCommand Send event:[50] AM ! RLC_AM_DATA_REQ = PDU (view PDU) Attach:[27] Exit Test Step ts_RRC_Security::lt_SendSecurityModeCommand
00:01:43.890 - Primitive: RLC_AM_DATA_IND: securityModeComplete 00:01:43.890 - Primitive: RLC_AM_DATA_IND begin "car_RRC_SecModeCmpl" of type RLC_AM_DATA_IND (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "integrityResult" of type IntegrityResult (CHOICE) [UNIVERSAL 31] matching [integrityUsed: i_pass] against * end "integrityResult" of type IntegrityResult begin "aM_message" of type CHOICE [UNIVERSAL 31] begin "uL_DCCH_Message" of type UL_DCCH_Message (SEQUENCE) [UNIVERSAL 16] begin "integrityCheckInfo" of type IntegrityCheckInfo (SEQUENCE) [UNIVERSAL 16] matching { messageAuthenticationCode: '00001110011110111110000111111100'B , rrc_MessageSequenceNumber: 1 } against * end "integrityCheckInfo" of type IntegrityCheckInfo begin "message" of type UL_DCCH_MessageType (CHOICE) [UNIVERSAL 31] begin "securityModeComplete" of type SecurityModeComplete (SEQUENCE) [UNIVERSAL 16] begin "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier (INTEGER) [UNIVERSAL 2] matching 0 against 0 end "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier begin "ul_IntegProtActivationInfo" of type IntegrityProtActivationInfo (SEQUENCE) [UNIVERSAL 16] matching { rrc_MessageSequenceNumberList: [ 0 , 0 , 0 , 0 , 0 ] } against * end "ul_IntegProtActivationInfo" of type IntegrityProtActivationInfo begin "rb_UL_CiphActivationTimeInfo" of type RB_ActivationTimeInfoList (SEQUENCEOF) [UNIVERSAL 28] matching [ { rb_Identity: 1 , rlc_SequenceNumber: 0 } , { rb_Identity: 2 , rlc_SequenceNumber: 7 } , { rb_Identity: 3 , rlc_SequenceNumber: 4 } , { rb_Identity: 4 , rlc_SequenceNumber: 0 } ] against ? end "rb_UL_CiphActivationTimeInfo" of type RB_ActivationTimeInfoList end "securityModeComplete" of type SecurityModeComplete end "message" of type UL_DCCH_MessageType end "uL_DCCH_Message" of type UL_DCCH_Message end "aM_message" of type CHOICE end "car_RRC_SecModeCmpl" of type RLC_AM_DATA_IND Assignment:TSP1: [29] uL_Integrity := { rrc_MessageSequenceNumberList: [ 0 , 0 , 0 , 0 , 0 ] } Assignment:TSP1: [29] uL_CipherMode := (view Assignment) Receive event:TSP1: [29] AM ? RLC_AM_DATA_IND = PDU (view PDU) Preliminary verdict:TSP1: [29] (PASS) Attach:[30] Enter Test Step ts_CRLC_UL_CipherCfg( [ { rb_Identity: 1 , r ...
| (view Test Step parameters) 00:01:43.890 - Primitive: CRLC_Ciphering_Activate_REQ Send event:[1] CRLC ! CRLC_Ciphering_Activate_REQ = PDU (view PDU) 00:01:44.130 - Primitive: RLC_AM_DATA_IND: uplinkDirectTransfer 00:01:44.130 - Primitive: RRC_DATA_IND: cc:setup 00:01:44.180 - Primitive: CRLC_Ciphering_Activate_CNF begin "ca_CRLC_CipherActCnf" of type CRLC_Ciphering_Activate_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER end "ca_CRLC_CipherActCnf" of type CRLC_Ciphering_Activate_CNF Receive event:[2] CRLC ? CRLC_Ciphering_Activate_CNF = PDU: { cellId: -1 } Attach:[30] Exit Test Step ts_CRLC_UL_CipherCfg
Attach:[31] Enter Test Step ts_CRLC_UL_Integrity( { rrc_MessageSequenceNumberList: [ 0 , 0 , 0 , 0 , 0 ] } )
| 00:01:44.180 - Primitive: CRLC_Integrity_Activate_REQ Send event:[1] CRLC ! CRLC_Integrity_Activate_REQ = PDU (view PDU) begin "car_PS_InitDirectTransfer" of type RRC_DataInd (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "rB_Id" of type SS_RB_Identity (INTEGER) [UNIVERSAL 2] matching 3 against 3 end "rB_Id" of type SS_RB_Identity begin "cN_Domain" of type SS_CN_DomainIdentity (INTEGER) [UNIVERSAL 2] matching 0 against 1 end "cN_Domain" of type SS_CN_DomainIdentity end "car_PS_InitDirectTransfer" of type RRC_DataInd Match failed [#1] : (view details)
Expected | RRC_DataInd
Received | RRC_DataInd
begin "car_InitDirectTransfer" of type RRC_DataInd (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "rB_Id" of type SS_RB_Identity (INTEGER) [UNIVERSAL 2] matching 3 against 3 end "rB_Id" of type SS_RB_Identity begin "cN_Domain" of type SS_CN_DomainIdentity (INTEGER) [UNIVERSAL 2] matching 0 against 0 end "cN_Domain" of type SS_CN_DomainIdentity matching OMIT against ? end "car_InitDirectTransfer" of type RRC_DataInd Match failed [#2] : (view details)
Expected | RRC_DataInd
Received | RRC_DataInd
begin "car_PS_InitDirectTransfer" of type RRC_DataInd (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "rB_Id" of type SS_RB_Identity (INTEGER) [UNIVERSAL 2] matching 3 against 3 end "rB_Id" of type SS_RB_Identity begin "cN_Domain" of type SS_CN_DomainIdentity (INTEGER) [UNIVERSAL 2] matching 0 against 1 end "cN_Domain" of type SS_CN_DomainIdentity end "car_PS_InitDirectTransfer" of type RRC_DataInd Match failed [#3] : (view details)
Expected | RRC_DataInd
Received | RRC_DataInd
00:01:44.190 - Primitive: CRLC_Integrity_Activate_CNF begin "ca_CRLC_IntegrityActivateCnf" of type CRLC_Integrity_Activate_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER end "ca_CRLC_IntegrityActivateCnf" of type CRLC_Integrity_Activate_CNF Receive event:[2] CRLC ? CRLC_Integrity_Activate_CNF = PDU: { cellId: -1 } Attach:[31] Exit Test Step ts_CRLC_UL_Integrity
Attach:[6] Exit Test Step ts_RRC_Security::lt_StartSecurity_UE
Attach:[8] Enter Test Step ts_CRLC_ResumeSecurity( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
00:01:44.190 - Primitive: CRLC_Resume_REQ Send event:[2] CRLC ! CRLC_Resume_REQ = PDU: { cellId: -1 , routingInfo: [rB_Identity: 1 ]} begin "car_PS_InitDirectTransfer" of type RRC_DataInd (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "rB_Id" of type SS_RB_Identity (INTEGER) [UNIVERSAL 2] matching 3 against 3 end "rB_Id" of type SS_RB_Identity begin "cN_Domain" of type SS_CN_DomainIdentity (INTEGER) [UNIVERSAL 2] matching 0 against 1 end "cN_Domain" of type SS_CN_DomainIdentity end "car_PS_InitDirectTransfer" of type RRC_DataInd Match failed [#4] : (view details)
Expected | RRC_DataInd
Received | RRC_DataInd
begin "car_InitDirectTransfer" of type RRC_DataInd (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "rB_Id" of type SS_RB_Identity (INTEGER) [UNIVERSAL 2] matching 3 against 3 end "rB_Id" of type SS_RB_Identity begin "cN_Domain" of type SS_CN_DomainIdentity (INTEGER) [UNIVERSAL 2] matching 0 against 0 end "cN_Domain" of type SS_CN_DomainIdentity matching OMIT against ? end "car_InitDirectTransfer" of type RRC_DataInd Match failed [#5] : (view details)
Expected | RRC_DataInd
Received | RRC_DataInd
begin "car_PS_InitDirectTransfer" of type RRC_DataInd (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "rB_Id" of type SS_RB_Identity (INTEGER) [UNIVERSAL 2] matching 3 against 3 end "rB_Id" of type SS_RB_Identity begin "cN_Domain" of type SS_CN_DomainIdentity (INTEGER) [UNIVERSAL 2] matching 0 against 1 end "cN_Domain" of type SS_CN_DomainIdentity end "car_PS_InitDirectTransfer" of type RRC_DataInd Match failed [#6] : (view details)
Expected | RRC_DataInd
Received | RRC_DataInd
begin "car_PS_InitDirectTransfer" of type RRC_DataInd (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "rB_Id" of type SS_RB_Identity (INTEGER) [UNIVERSAL 2] matching 3 against 3 end "rB_Id" of type SS_RB_Identity begin "cN_Domain" of type SS_CN_DomainIdentity (INTEGER) [UNIVERSAL 2] matching 0 against 1 end "cN_Domain" of type SS_CN_DomainIdentity end "car_PS_InitDirectTransfer" of type RRC_DataInd Match failed [#7] : (view details)
Expected | RRC_DataInd
Received | RRC_DataInd
begin "car_InitDirectTransfer" of type RRC_DataInd (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "rB_Id" of type SS_RB_Identity (INTEGER) [UNIVERSAL 2] matching 3 against 3 end "rB_Id" of type SS_RB_Identity begin "cN_Domain" of type SS_CN_DomainIdentity (INTEGER) [UNIVERSAL 2] matching 0 against 0 end "cN_Domain" of type SS_CN_DomainIdentity matching OMIT against ? end "car_InitDirectTransfer" of type RRC_DataInd Match failed [#8] : (view details)
Expected | RRC_DataInd
Received | RRC_DataInd
begin "car_PS_InitDirectTransfer" of type RRC_DataInd (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "rB_Id" of type SS_RB_Identity (INTEGER) [UNIVERSAL 2] matching 3 against 3 end "rB_Id" of type SS_RB_Identity begin "cN_Domain" of type SS_CN_DomainIdentity (INTEGER) [UNIVERSAL 2] matching 0 against 1 end "cN_Domain" of type SS_CN_DomainIdentity end "car_PS_InitDirectTransfer" of type RRC_DataInd Match failed [#9] : (view details)
Expected | RRC_DataInd
Received | RRC_DataInd
00:01:44.220 - Primitive: CRLC_Resume_CNF begin "car_ResumeRB" of type CRLC_Resume_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "car_ResumeRB" of type CRLC_Resume_CNF Receive event:[3] CRLC ? CRLC_Resume_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 1 ]} 00:01:44.220 - Primitive: CRLC_Resume_REQ Send event:[4] CRLC ! CRLC_Resume_REQ = PDU: { cellId: -1 , routingInfo: [rB_Identity: 3 ]} begin "car_PS_InitDirectTransfer" of type RRC_DataInd (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "rB_Id" of type SS_RB_Identity (INTEGER) [UNIVERSAL 2] matching 3 against 3 end "rB_Id" of type SS_RB_Identity begin "cN_Domain" of type SS_CN_DomainIdentity (INTEGER) [UNIVERSAL 2] matching 0 against 1 end "cN_Domain" of type SS_CN_DomainIdentity end "car_PS_InitDirectTransfer" of type RRC_DataInd Match failed [#10] : (view details)
Expected | RRC_DataInd
Received | RRC_DataInd
begin "car_InitDirectTransfer" of type RRC_DataInd (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "rB_Id" of type SS_RB_Identity (INTEGER) [UNIVERSAL 2] matching 3 against 3 end "rB_Id" of type SS_RB_Identity begin "cN_Domain" of type SS_CN_DomainIdentity (INTEGER) [UNIVERSAL 2] matching 0 against 0 end "cN_Domain" of type SS_CN_DomainIdentity matching OMIT against ? end "car_InitDirectTransfer" of type RRC_DataInd Match failed [#11] : (view details)
Expected | RRC_DataInd
Received | RRC_DataInd
begin "car_PS_InitDirectTransfer" of type RRC_DataInd (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "rB_Id" of type SS_RB_Identity (INTEGER) [UNIVERSAL 2] matching 3 against 3 end "rB_Id" of type SS_RB_Identity begin "cN_Domain" of type SS_CN_DomainIdentity (INTEGER) [UNIVERSAL 2] matching 0 against 1 end "cN_Domain" of type SS_CN_DomainIdentity end "car_PS_InitDirectTransfer" of type RRC_DataInd Match failed [#12] : (view details)
Expected | RRC_DataInd
Received | RRC_DataInd
begin "car_PS_InitDirectTransfer" of type RRC_DataInd (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "rB_Id" of type SS_RB_Identity (INTEGER) [UNIVERSAL 2] matching 3 against 3 end "rB_Id" of type SS_RB_Identity begin "cN_Domain" of type SS_CN_DomainIdentity (INTEGER) [UNIVERSAL 2] matching 0 against 1 end "cN_Domain" of type SS_CN_DomainIdentity end "car_PS_InitDirectTransfer" of type RRC_DataInd Match failed [#13] : (view details)
Expected | RRC_DataInd
Received | RRC_DataInd
begin "car_InitDirectTransfer" of type RRC_DataInd (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "rB_Id" of type SS_RB_Identity (INTEGER) [UNIVERSAL 2] matching 3 against 3 end "rB_Id" of type SS_RB_Identity begin "cN_Domain" of type SS_CN_DomainIdentity (INTEGER) [UNIVERSAL 2] matching 0 against 0 end "cN_Domain" of type SS_CN_DomainIdentity matching OMIT against ? end "car_InitDirectTransfer" of type RRC_DataInd Match failed [#14] : (view details)
Expected | RRC_DataInd
Received | RRC_DataInd
begin "car_PS_InitDirectTransfer" of type RRC_DataInd (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "rB_Id" of type SS_RB_Identity (INTEGER) [UNIVERSAL 2] matching 3 against 3 end "rB_Id" of type SS_RB_Identity begin "cN_Domain" of type SS_CN_DomainIdentity (INTEGER) [UNIVERSAL 2] matching 0 against 1 end "cN_Domain" of type SS_CN_DomainIdentity end "car_PS_InitDirectTransfer" of type RRC_DataInd Match failed [#15] : (view details)
Expected | RRC_DataInd
Received | RRC_DataInd
00:01:44.250 - Primitive: CRLC_Resume_CNF begin "car_ResumeRB" of type CRLC_Resume_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "car_ResumeRB" of type CRLC_Resume_CNF Receive event:[5] CRLC ? CRLC_Resume_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 3 ]} 00:01:44.250 - Primitive: CRLC_Resume_REQ Send event:[6] CRLC ! CRLC_Resume_REQ = PDU: { cellId: -1 , routingInfo: [rB_Identity: 4 ]} begin "car_PS_InitDirectTransfer" of type RRC_DataInd (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "rB_Id" of type SS_RB_Identity (INTEGER) [UNIVERSAL 2] matching 3 against 3 end "rB_Id" of type SS_RB_Identity begin "cN_Domain" of type SS_CN_DomainIdentity (INTEGER) [UNIVERSAL 2] matching 0 against 1 end "cN_Domain" of type SS_CN_DomainIdentity end "car_PS_InitDirectTransfer" of type RRC_DataInd Match failed [#16] : (view details)
Expected | RRC_DataInd
Received | RRC_DataInd
begin "car_InitDirectTransfer" of type RRC_DataInd (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "rB_Id" of type SS_RB_Identity (INTEGER) [UNIVERSAL 2] matching 3 against 3 end "rB_Id" of type SS_RB_Identity begin "cN_Domain" of type SS_CN_DomainIdentity (INTEGER) [UNIVERSAL 2] matching 0 against 0 end "cN_Domain" of type SS_CN_DomainIdentity matching OMIT against ? end "car_InitDirectTransfer" of type RRC_DataInd Match failed [#17] : (view details)
Expected | RRC_DataInd
Received | RRC_DataInd
begin "car_PS_InitDirectTransfer" of type RRC_DataInd (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "rB_Id" of type SS_RB_Identity (INTEGER) [UNIVERSAL 2] matching 3 against 3 end "rB_Id" of type SS_RB_Identity begin "cN_Domain" of type SS_CN_DomainIdentity (INTEGER) [UNIVERSAL 2] matching 0 against 1 end "cN_Domain" of type SS_CN_DomainIdentity end "car_PS_InitDirectTransfer" of type RRC_DataInd Match failed [#18] : (view details)
Expected | RRC_DataInd
Received | RRC_DataInd
begin "car_PS_InitDirectTransfer" of type RRC_DataInd (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "rB_Id" of type SS_RB_Identity (INTEGER) [UNIVERSAL 2] matching 3 against 3 end "rB_Id" of type SS_RB_Identity begin "cN_Domain" of type SS_CN_DomainIdentity (INTEGER) [UNIVERSAL 2] matching 0 against 1 end "cN_Domain" of type SS_CN_DomainIdentity end "car_PS_InitDirectTransfer" of type RRC_DataInd Match failed [#19] : (view details)
Expected | RRC_DataInd
Received | RRC_DataInd
begin "car_InitDirectTransfer" of type RRC_DataInd (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "rB_Id" of type SS_RB_Identity (INTEGER) [UNIVERSAL 2] matching 3 against 3 end "rB_Id" of type SS_RB_Identity begin "cN_Domain" of type SS_CN_DomainIdentity (INTEGER) [UNIVERSAL 2] matching 0 against 0 end "cN_Domain" of type SS_CN_DomainIdentity matching OMIT against ? end "car_InitDirectTransfer" of type RRC_DataInd Match failed [#20] : (view details)
Expected | RRC_DataInd
Received | RRC_DataInd
begin "car_PS_InitDirectTransfer" of type RRC_DataInd (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "rB_Id" of type SS_RB_Identity (INTEGER) [UNIVERSAL 2] matching 3 against 3 end "rB_Id" of type SS_RB_Identity begin "cN_Domain" of type SS_CN_DomainIdentity (INTEGER) [UNIVERSAL 2] matching 0 against 1 end "cN_Domain" of type SS_CN_DomainIdentity end "car_PS_InitDirectTransfer" of type RRC_DataInd Match failed [#21] : (view details)
Expected | RRC_DataInd
Received | RRC_DataInd
00:01:44.290 - Primitive: CRLC_Resume_CNF begin "car_ResumeRB" of type CRLC_Resume_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "car_ResumeRB" of type CRLC_Resume_CNF Assignment:[7] tcv_RB_SigResumed := GcTRUE Receive event:[7] CRLC ? CRLC_Resume_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 4 ]} Attach:[8] Exit Test Step ts_CRLC_ResumeSecurity
Attach:[2] Exit Test Step ts_RRC_Security
Attach:[3] Enter Test Step ts_CC_RcvSetupOrEsetup( 0 )
| Attach:[2] Enter Test Step ts_CC_RcvSetupOrEsetup::lt_CC_TelephonyMO( 0 )
| begin "car_UplinkDirectTransfer" of type RRC_DataInd (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "rB_Id" of type SS_RB_Identity (INTEGER) [UNIVERSAL 2] matching 3 against 3 end "rB_Id" of type SS_RB_Identity begin "cN_Domain" of type SS_CN_DomainIdentity (INTEGER) [UNIVERSAL 2] matching 0 against 0 end "cN_Domain" of type SS_CN_DomainIdentity begin "msg" of type SETUPul (SEQUENCE) [UNIVERSAL 16] begin "ti" of type TI (SEQUENCE) [UNIVERSAL 16] begin "tiFlag" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against '0'B end "tiFlag" of type B1 begin "tiVal" of type B3 (BITSTRING) [UNIVERSAL 3] matching '000'B against ? end "tiVal" of type B3 end "ti" of type TI begin "cC_ProtocolDiscriminator" of type ProtocolDiscriminator (BITSTRING) [UNIVERSAL 3] matching '0011'B against '0011'B end "cC_ProtocolDiscriminator" of type ProtocolDiscriminator begin "msgType" of type MsgType (BITSTRING) [UNIVERSAL 3] matching '10000101'B against '??000101'B end "msgType" of type MsgType begin "bcap1" of type Bcap (SEQUENCE) [UNIVERSAL 16] begin "iei" of type IEI8 (BITSTRING) [UNIVERSAL 3] matching '00000100'B against '00000100'B end "iei" of type IEI8 begin "iel" of type Length (OCTETSTRING) [UNIVERSAL 4] matching '03'O against ? end "iel" of type Length begin "extBit3" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against ? end "extBit3" of type B1 begin "radioChRequi" of type B2 (BITSTRING) [UNIVERSAL 3] matching '01'B against ? end "radioChRequi" of type B2 begin "codingStd" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against '0'B end "codingStd" of type B1 begin "transferMode" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against '0'B end "transferMode" of type B1 begin "itc" of type B3 (BITSTRING) [UNIVERSAL 3] matching '000'B against '000'B end "itc" of type B3 begin "bcap3aEtc1" of type Bcap3aEtc (SEQUENCE) [UNIVERSAL 16] begin "extBit" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against * end "extBit" of type B1 begin "coding" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against * end "coding" of type B1 begin "spare2" of type B2 (BITSTRING) [UNIVERSAL 3] matching '00'B against * end "spare2" of type B2 begin "speechVersion" of type B4 (BITSTRING) [UNIVERSAL 3] matching '0010'B against * end "speechVersion" of type B4 end "bcap3aEtc1" of type Bcap3aEtc begin "bcap3aEtc2" of type Bcap3aEtc (SEQUENCE) [UNIVERSAL 16] begin "extBit" of type B1 (BITSTRING) [UNIVERSAL 3] matching '1'B against * end "extBit" of type B1 begin "coding" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against * end "coding" of type B1 begin "spare2" of type B2 (BITSTRING) [UNIVERSAL 3] matching '00'B against * end "spare2" of type B2 begin "speechVersion" of type B4 (BITSTRING) [UNIVERSAL 3] matching '0000'B against * end "speechVersion" of type B4 end "bcap3aEtc2" of type Bcap3aEtc end "bcap1" of type Bcap begin "cdpn" of type CDPN (SEQUENCE) [UNIVERSAL 16] begin "iei" of type IEI8 (BITSTRING) [UNIVERSAL 3] matching '01011110'B against '01011110'B end "iei" of type IEI8 begin "iel" of type Length (OCTETSTRING) [UNIVERSAL 4] matching '03'O against ? end "iel" of type Length begin "typeOfNumPlan" of type TypeOfNumPlan (SEQUENCE) [UNIVERSAL 16] begin "extBit" of type B1 (BITSTRING) [UNIVERSAL 3] matching '1'B against ? end "extBit" of type B1 begin "typeOfNum" of type B3 (BITSTRING) [UNIVERSAL 3] matching '000'B against ? end "typeOfNum" of type B3 begin "numbPlanId" of type B4 (BITSTRING) [UNIVERSAL 3] matching '0001'B against ? end "numbPlanId" of type B4 end "typeOfNumPlan" of type TypeOfNumPlan begin "digits" of type OCTETSTRING [UNIVERSAL 4] matching '21F3'O against * end "digits" of type OCTETSTRING end "cdpn" of type CDPN begin "cC_Capabilities" of type CC_Capabilities (SEQUENCE) [UNIVERSAL 16] begin "iei" of type IEI8 (BITSTRING) [UNIVERSAL 3] matching '00010101'B against '00010101'B end "iei" of type IEI8 begin "iel" of type Length (OCTETSTRING) [UNIVERSAL 4] matching '02'O against ? end "iel" of type Length begin "maxNumBearer" of type B4 (BITSTRING) [UNIVERSAL 3] matching '0000'B against * end "maxNumBearer" of type B4 begin "spare2" of type B2 (BITSTRING) [UNIVERSAL 3] matching '00'B against * end "spare2" of type B2 begin "pcp" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against * end "pcp" of type B1 begin "dtmf" of type B1 (BITSTRING) [UNIVERSAL 3] matching '1'B against * end "dtmf" of type B1 begin "spare4" of type B4 (BITSTRING) [UNIVERSAL 3] matching '0000'B against * end "spare4" of type B4 begin "maxNumSpeechBearer" of type B4 (BITSTRING) [UNIVERSAL 3] matching '0001'B against * end "maxNumSpeechBearer" of type B4 end "cC_Capabilities" of type CC_Capabilities end "msg" of type SETUPul end "car_UplinkDirectTransfer" of type RRC_DataInd Assignment:[21] tcv_SetupMOr := PDU (view PDU) Receive event:[21] Dc ? RRC_DataInd = PDU (view PDU) Attach:[2] Exit Test Step ts_CC_RcvSetupOrEsetup::lt_CC_TelephonyMO
Attach:[3] Enter Test Step ts_CC_RcvSetupOrEsetup::lt_InitCC_tcv( 0 )
| Assignment:[17] tcv_TI_R := { tiFlag: '0'B , tiVal: '000'B } Assignment:[17] tcv_TI_S := { tiFlag: '0'B , tiVal: '000'B } Assignment:[17] tiFlag := '1'B Assignment:[17] tcv_RAB_Id := '00000001'B Attach:[3] Exit Test Step ts_CC_RcvSetupOrEsetup::lt_InitCC_tcv
Attach:[3] Exit Test Step ts_CC_RcvSetupOrEsetup
00:01:44.290 - Primitive: RRC_DATA_REQ: cc:callProceeding 00:01:44.290 - Primitive: RLC_AM_DATA_REQ:downlinkDirectTransfer Send event:[4] Dc ! RRC_DataReq = PDU (view PDU) Attach:[8] Exit Test Step ts_RRC_NAS_CallSetupCS_MO_P7_P8
Attach:[9] Enter Test Step ts_RRC_RAB_EstCS_MO_P11_P12( 0 )
| Attach:[1] Enter Test Step ts_RRC_SetUpRAB( 0 )
| Attach:[1] Enter Test Step ts_CalculateActTime( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[3] Enter Test Step ts_CPHY_ActTime( 0 )
| 00:01:44.300 - Primitive: CPHY_Frame_Number_REQ Send event:[1] CPHY ! CPHY_Frame_Number_REQ = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 26 ]} 00:01:44.410 - Primitive: CPHY_Frame_Number_CNF begin "car_GetFrameNum" of type CPHY_Frame_Number_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 26 against 26 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo begin "frameNumber" of type INTEGER [UNIVERSAL 2] matching 208 against ? end "frameNumber" of type INTEGER end "car_GetFrameNum" of type CPHY_Frame_Number_CNF Assignment:[2] tcv_FrameNumber := 208 Receive event:[2] CPHY ? CPHY_Frame_Number_CNF = PDU (view PDU) Assignment:[3] tcv_ActTime := 200 Assignment:[3] tcv_TGCFN := 204 Attach:[3] Exit Test Step ts_CPHY_ActTime
Attach:[1] Exit Test Step ts_CalculateActTime
Attach:[3] Enter Test Step ts_RRC_SendRB_SetUpDCH_Speech( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
00:01:44.410 - Primitive: RLC_AM_DATA_REQ 00:01:44.430 - Primitive: RLC_AM_DATA_REQ: radioBearerSetup Send event:[2] AM ! RLC_AM_DATA_REQ = PDU (view PDU) 00:01:44.880 - Primitive: RLC_AM_DATA_CNF begin "car_AM_DataMuiCnf" of type RLC_AM_DATA_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "mui" of type Mui (INTEGER) [UNIVERSAL 2] matching 0 against 0 end "mui" of type Mui end "car_AM_DataMuiCnf" of type RLC_AM_DATA_CNF Receive event:[3] AM ? RLC_AM_DATA_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 2 ], mui: 0 } Attach:[4] Enter Test Step ts_SS_4DCH_Modify( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
00:01:44.880 - Primitive: CPHY_RL_Modify_REQ Send event:[3] CPHY ! CPHY_RL_Modify_REQ = PDU (view PDU) 00:01:45.080 - Primitive: CPHY_RL_Modify_CNF begin "ca_RL_ModifyCnf" of type CPHY_RL_Modify_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 26 against 26 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_ModifyCnf" of type CPHY_RL_Modify_CNF Receive event:[4] CPHY ? CPHY_RL_Modify_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 26 ]} 00:01:45.080 - Primitive: CPHY_TrCH_Config_REQ Send event:[5] CPHY ! CPHY_TrCH_Config_REQ = PDU (view PDU) 00:01:45.110 - Primitive: CPHY_TrCH_Config_CNF begin "ca_TrChCfgCnf" of type CPHY_TrCH_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 26 against 26 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_TrChCfgCnf" of type CPHY_TrCH_Config_CNF Receive event:[6] CPHY ? CPHY_TrCH_Config_CNF = PDU (view PDU) 00:01:45.110 - Primitive: CMAC_Config_REQ Send event:[7] CMAC ! CMAC_Config_REQ = PDU (view PDU) 00:01:45.140 - Primitive: CMAC_Config_CNF begin "ca_CMAC_CfgCnf" of type CMAC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 26 against 26 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_CfgCnf" of type CMAC_Config_CNF Receive event:[8] CMAC ? CMAC_Config_CNF = PDU: { cellId: -1 , routingInfo: [physicalChannelIdentity: 26 ]} 00:01:45.140 - Primitive: CPHY_RL_Modify_REQ Send event:[9] CPHY ! CPHY_RL_Modify_REQ = PDU (view PDU) 00:01:45.290 - Primitive: CPHY_RL_Modify_CNF begin "ca_RL_ModifyCnf" of type CPHY_RL_Modify_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 20 against 20 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_ModifyCnf" of type CPHY_RL_Modify_CNF Receive event:[10] CPHY ? CPHY_RL_Modify_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 20 ]} 00:01:45.290 - Primitive: CPHY_TrCH_Config_REQ Send event:[11] CPHY ! CPHY_TrCH_Config_REQ = PDU (view PDU) 00:01:45.390 - Primitive: CPHY_TrCH_Config_CNF begin "ca_TrChCfgCnf" of type CPHY_TrCH_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 20 against 20 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_TrChCfgCnf" of type CPHY_TrCH_Config_CNF Receive event:[12] CPHY ? CPHY_TrCH_Config_CNF = PDU (view PDU) 00:01:45.390 - Primitive: CMAC_Config_REQ Send event:[13] CMAC ! CMAC_Config_REQ = PDU (view PDU) 00:01:45.440 - Primitive: CMAC_Config_CNF begin "ca_CMAC_CfgCnf" of type CMAC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 20 against 20 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_CfgCnf" of type CMAC_Config_CNF Receive event:[14] CMAC ? CMAC_Config_CNF = PDU: { cellId: -1 , routingInfo: [physicalChannelIdentity: 20 ]} Attach:[4] Exit Test Step ts_SS_4DCH_Modify
Attach:[5] Enter Test Step ts_SS_RB10_ToRB12_TM_Cfg( )
| 00:01:45.440 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:45.520 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 10 against 10 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 10 ]} 00:01:45.520 - Primitive: CRLC_Config_REQ Send event:[3] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:45.690 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 11 against 11 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[4] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 11 ]} 00:01:45.690 - Primitive: CRLC_Config_REQ Send event:[5] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:01:45.740 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 12 against 12 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[6] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 12 ]} Attach:[5] Exit Test Step ts_SS_RB10_ToRB12_TM_Cfg
Attach:TSP: [6] Enter Test Step ts_RRC_ReceiveRB_SetupCmpl( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
StartTimer:[2] t_WaitMS [13500] 13500 ms Attach:[5] Enter Test Step ts_RRC_ReceiveRB_SetupCmpl::lt_CipheringStartedTM_RAB( 0 )
| Attach:[13] Enter Test Step ts_CMAC_DownloadSecurityKey( '010001000111011101100 ...
| (view Test Step parameters) 00:01:45.740 - Primitive: CMAC_SecurityMode_Config_REQ Send event:[1] CMAC ! CMAC_SecurityMode_Config_REQ = PDU (view PDU) 00:01:45.750 - Primitive: CMAC_SecurityMode_Config_CNF begin "ca_CMAC_SecurityModeCfgCnf" of type CMAC_SecurityMode_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER end "ca_CMAC_SecurityModeCfgCnf" of type CMAC_SecurityMode_Config_CNF Receive event:[2] CMAC ? CMAC_SecurityMode_Config_CNF = PDU: { cellId: -1 } Attach:[13] Exit Test Step ts_CMAC_DownloadSecurityKey
Attach:[14] Enter Test Step ts_CMAC_UL_DL_CipherCfg( [startRestart: uea0] )
| Attach:[1] Enter Test Step ts_CMAC_DL_CipherCfg( [startRestart: uea0] )
| 00:01:45.750 - Primitive: CMAC_Ciphering_Activate_REQ Send event:[1] CMAC ! CMAC_Ciphering_Activate_REQ = PDU (view PDU) 00:01:45.770 - Primitive: CMAC_Ciphering_Activate_CNF begin "ca_CMAC_CipherActCnf" of type CMAC_Ciphering_Activate_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 26 against 26 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_CipherActCnf" of type CMAC_Ciphering_Activate_CNF Receive event:[2] CMAC ? CMAC_Ciphering_Activate_CNF = PDU (view PDU) Attach:[1] Exit Test Step ts_CMAC_DL_CipherCfg
Attach:[2] Enter Test Step ts_CMAC_UL_CipherCfg( [startRestart: uea0] )
| 00:01:45.770 - Primitive: CMAC_Ciphering_Activate_REQ Send event:[1] CMAC ! CMAC_Ciphering_Activate_REQ = PDU (view PDU) 00:01:45.790 - Primitive: CMAC_Ciphering_Activate_CNF begin "ca_CMAC_CipherActCnf" of type CMAC_Ciphering_Activate_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 20 against 20 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_CipherActCnf" of type CMAC_Ciphering_Activate_CNF Receive event:[2] CMAC ? CMAC_Ciphering_Activate_CNF = PDU (view PDU) Attach:[2] Exit Test Step ts_CMAC_UL_CipherCfg
Attach:[14] Exit Test Step ts_CMAC_UL_DL_CipherCfg
00:01:47.140 - Primitive: RLC_AM_DATA_IND: radioBearerSetupComplete 00:01:47.140 - Primitive: RLC_AM_DATA_IND begin "car_RB_SetUpCmpl" of type RLC_AM_DATA_IND (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "integrityResult" of type IntegrityResult (CHOICE) [UNIVERSAL 31] matching [integrityUsed: i_pass] against * end "integrityResult" of type IntegrityResult begin "aM_message" of type CHOICE [UNIVERSAL 31] begin "uL_DCCH_Message" of type UL_DCCH_Message (SEQUENCE) [UNIVERSAL 16] begin "integrityCheckInfo" of type IntegrityCheckInfo (SEQUENCE) [UNIVERSAL 16] matching { messageAuthenticationCode: '10111100111100100110010000101011'B , rrc_MessageSequenceNumber: 2 } against * end "integrityCheckInfo" of type IntegrityCheckInfo begin "message" of type UL_DCCH_MessageType (CHOICE) [UNIVERSAL 31] begin "radioBearerSetupComplete" of type RadioBearerSetupComplete (SEQUENCE) [UNIVERSAL 16] begin "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier (INTEGER) [UNIVERSAL 2] matching 0 against 0 end "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier begin "start_Value" of type START_Value (BITSTRING) [UNIVERSAL 3] matching '00000000000000000010'B against * end "start_Value" of type START_Value begin "count_C_ActivationTime" of type ActivationTime (INTEGER) [UNIVERSAL 2] matching 184 against * end "count_C_ActivationTime" of type ActivationTime end "radioBearerSetupComplete" of type RadioBearerSetupComplete end "message" of type UL_DCCH_MessageType end "uL_DCCH_Message" of type UL_DCCH_Message end "aM_message" of type CHOICE end "car_RB_SetUpCmpl" of type RLC_AM_DATA_IND Assignment:TSP2: [16] tcv_CipherActTime := 184 Assignment:TSP2: [16] start_CS := '00000000000000000010'B CancelTimer:TSP2: [16] t_WaitMS [13500] 13500 ms Receive event:TSP2: [16] AM ? RLC_AM_DATA_IND = PDU (view PDU) Preliminary verdict:TSP2: [16] (PASS) Attach:[17] Enter Test Step ts_CMAC_DownloadSecurityKey( '010001000111011101100 ...
| (view Test Step parameters) 00:01:47.140 - Primitive: CMAC_SecurityMode_Config_REQ Send event:[1] CMAC ! CMAC_SecurityMode_Config_REQ = PDU (view PDU) 00:01:47.160 - Primitive: CMAC_SecurityMode_Config_CNF begin "ca_CMAC_SecurityModeCfgCnf" of type CMAC_SecurityMode_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER end "ca_CMAC_SecurityModeCfgCnf" of type CMAC_SecurityMode_Config_CNF Receive event:[2] CMAC ? CMAC_SecurityMode_Config_CNF = PDU: { cellId: -1 } Attach:[17] Exit Test Step ts_CMAC_DownloadSecurityKey
Attach:[18] Enter Test Step ts_CMAC_UL_DL_CipherCfg( [startRestart: uea0] )
| Attach:[1] Enter Test Step ts_CMAC_DL_CipherCfg( [startRestart: uea0] )
| 00:01:47.160 - Primitive: CMAC_Ciphering_Activate_REQ Send event:[1] CMAC ! CMAC_Ciphering_Activate_REQ = PDU (view PDU) 00:01:47.180 - Primitive: CMAC_Ciphering_Activate_CNF begin "ca_CMAC_CipherActCnf" of type CMAC_Ciphering_Activate_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 26 against 26 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_CipherActCnf" of type CMAC_Ciphering_Activate_CNF Receive event:[2] CMAC ? CMAC_Ciphering_Activate_CNF = PDU (view PDU) Attach:[1] Exit Test Step ts_CMAC_DL_CipherCfg
Attach:[2] Enter Test Step ts_CMAC_UL_CipherCfg( [startRestart: uea0] )
| 00:01:47.180 - Primitive: CMAC_Ciphering_Activate_REQ Send event:[1] CMAC ! CMAC_Ciphering_Activate_REQ = PDU (view PDU) 00:01:47.190 - Primitive: CMAC_Ciphering_Activate_CNF begin "ca_CMAC_CipherActCnf" of type CMAC_Ciphering_Activate_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 20 against 20 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_CipherActCnf" of type CMAC_Ciphering_Activate_CNF Receive event:[2] CMAC ? CMAC_Ciphering_Activate_CNF = PDU (view PDU) Attach:[2] Exit Test Step ts_CMAC_UL_CipherCfg
Attach:[18] Exit Test Step ts_CMAC_UL_DL_CipherCfg
Attach:[5] Exit Test Step ts_RRC_ReceiveRB_SetupCmpl::lt_CipheringStartedTM_RAB
Attach:TSP: [6] Exit Test Step ts_RRC_ReceiveRB_SetupCmpl
Attach:[3] Exit Test Step ts_RRC_SendRB_SetUpDCH_Speech
Attach:[4] Enter Test Step ts_SetCellCfg( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Assignment:[2] cellConfig := cell_DCH_Speech Attach:[3] Enter Test Step ts_SaveCellInfo( 0 )
| Assignment:[2] tcv_CellInfoA := (view Assignment) Attach:[3] Exit Test Step ts_SaveCellInfo
Attach:[4] Exit Test Step ts_SetCellCfg
Attach:[1] Exit Test Step ts_RRC_SetUpRAB
Attach:[2] Enter Test Step ts_CC_SendAlertConnect( 0 )
| 00:01:47.190 - Primitive: RRC_DATA_REQ: cc:alerting 00:01:47.190 - Primitive: RLC_AM_DATA_REQ:downlinkDirectTransfer Send event:[1] Dc ! RRC_DataReq = PDU (view PDU) Attach:[2] Enter Test Step ts_CC_SendConnect( 0 )
| 00:01:47.190 - Primitive: RRC_DATA_REQ: cc:connect 00:01:47.190 - Primitive: RLC_AM_DATA_REQ:downlinkDirectTransfer Send event:[1] Dc ! RRC_DataReq = PDU (view PDU) 00:01:47.600 - Primitive: RLC_AM_DATA_IND: uplinkDirectTransfer 00:01:47.600 - Primitive: RRC_DATA_IND: cc:connectAcknowledge begin "car_UplinkDirectTransfer" of type RRC_DataInd (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "rB_Id" of type SS_RB_Identity (INTEGER) [UNIVERSAL 2] matching 3 against 3 end "rB_Id" of type SS_RB_Identity begin "cN_Domain" of type SS_CN_DomainIdentity (INTEGER) [UNIVERSAL 2] matching 0 against 0 end "cN_Domain" of type SS_CN_DomainIdentity begin "msg" of type CONNECTACKNOWLEDGE (SEQUENCE) [UNIVERSAL 16] begin "ti" of type TI (SEQUENCE) [UNIVERSAL 16] begin "tiFlag" of type B1 (BITSTRING) [UNIVERSAL 3] matching '0'B against '0'B end "tiFlag" of type B1 begin "tiVal" of type B3 (BITSTRING) [UNIVERSAL 3] matching '000'B against '000'B end "tiVal" of type B3 end "ti" of type TI begin "cC_ProtocolDiscriminator" of type ProtocolDiscriminator (BITSTRING) [UNIVERSAL 3] matching '0011'B against '0011'B end "cC_ProtocolDiscriminator" of type ProtocolDiscriminator begin "msgType" of type MsgType (BITSTRING) [UNIVERSAL 3] matching '11001111'B against '??001111'B end "msgType" of type MsgType end "msg" of type CONNECTACKNOWLEDGE end "car_UplinkDirectTransfer" of type RRC_DataInd Receive event:TSP: [2] Dc ? RRC_DataInd = PDU (view PDU) Preliminary verdict:TSP: [2] (PASS) Attach:[2] Exit Test Step ts_CC_SendConnect
Attach:[2] Exit Test Step ts_CC_SendAlertConnect
Attach:[9] Exit Test Step ts_RRC_RAB_EstCS_MO_P11_P12
Attach:[9] Exit Test Step ts_ToStateMO_CS_6_9_PS_6_10Or6_11
Attach:[10] Enter Test Step tc_8_4_1_25::lt_TestBody( )
| Assignment:TBS: [14] tcv_TestBody := GcTRUE 00:01:47.630 - Primitive: RLC_AM_DATA_REQ 00:01:47.630 - Primitive: RLC_AM_DATA_REQ: measurementControl Send event:[15] AM ! RLC_AM_DATA_REQ = PDU (view PDU) Attach:[16] Enter Test Step ts_PhyChannelReconfig_NoTFCI( dl_FrameTypeA )
| Attach:[1] Enter Test Step ts_CalculateActTime( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[3] Enter Test Step ts_CPHY_ActTime( 0 )
| 00:01:47.640 - Primitive: CPHY_Frame_Number_REQ Send event:[1] CPHY ! CPHY_Frame_Number_REQ = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 26 ]} 00:01:47.690 - Primitive: CPHY_Frame_Number_CNF begin "car_GetFrameNum" of type CPHY_Frame_Number_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 26 against 26 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo begin "frameNumber" of type INTEGER [UNIVERSAL 2] matching 25 against ? end "frameNumber" of type INTEGER end "car_GetFrameNum" of type CPHY_Frame_Number_CNF Assignment:[2] tcv_FrameNumber := 25 Receive event:[2] CPHY ? CPHY_Frame_Number_CNF = PDU (view PDU) Assignment:[3] tcv_ActTime := 16 Assignment:[3] tcv_TGCFN := 21 Attach:[3] Exit Test Step ts_CPHY_ActTime
Attach:[1] Exit Test Step ts_CalculateActTime
00:01:47.690 - Primitive: RLC_AM_DATA_REQ 00:01:47.690 - Primitive: RLC_AM_DATA_REQ: physicalChannelReconfiguration Send event:[4] AM ! RLC_AM_DATA_REQ = PDU (view PDU) 00:01:47.710 - Primitive: CPHY_RL_Modify_REQ Send event:[5] CPHY ! CPHY_RL_Modify_REQ = PDU (view PDU) 00:01:47.800 - Primitive: CPHY_RL_Modify_CNF begin "ca_CompressedModeInfoCNF" of type CPHY_RL_Modify_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 26 against 26 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CompressedModeInfoCNF" of type CPHY_RL_Modify_CNF Receive event:[6] CPHY ? CPHY_RL_Modify_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 26 ]} 00:01:47.800 - Primitive: CPHY_RL_Modify_REQ Send event:[7] CPHY ! CPHY_RL_Modify_REQ = PDU (view PDU) 00:01:48.000 - Primitive: CPHY_RL_Modify_CNF begin "ca_CompressedModeInfoCNF" of type CPHY_RL_Modify_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 20 against 20 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CompressedModeInfoCNF" of type CPHY_RL_Modify_CNF Receive event:[8] CPHY ? CPHY_RL_Modify_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 20 ]} Attach:[9] Enter Test Step ts_RRC_ReceivePhyChReconfCmpl( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
StartTimer:[2] t_WaitMS [13500] 13500 ms 00:01:50.640 - Primitive: RLC_AM_DATA_IND: physicalChannelReconfigurationComplete 00:01:50.640 - Primitive: RLC_AM_DATA_IND begin "car_PhyChReconfCmpl" of type RLC_AM_DATA_IND (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "integrityResult" of type IntegrityResult (CHOICE) [UNIVERSAL 31] matching [integrityUsed: i_pass] against ? end "integrityResult" of type IntegrityResult begin "aM_message" of type CHOICE [UNIVERSAL 31] begin "uL_DCCH_Message" of type UL_DCCH_Message (SEQUENCE) [UNIVERSAL 16] begin "integrityCheckInfo" of type IntegrityCheckInfo (SEQUENCE) [UNIVERSAL 16] matching { messageAuthenticationCode: '00010011111100011101100011010111'B , rrc_MessageSequenceNumber: 3 } against * end "integrityCheckInfo" of type IntegrityCheckInfo begin "message" of type UL_DCCH_MessageType (CHOICE) [UNIVERSAL 31] begin "physicalChannelReconfigurationComplete" of type PhysicalChannelReconfigurationComplete (SEQUENCE) [UNIVERSAL 16] begin "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier (INTEGER) [UNIVERSAL 2] matching 0 against 0 end "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier end "physicalChannelReconfigurationComplete" of type PhysicalChannelReconfigurationComplete end "message" of type UL_DCCH_MessageType end "uL_DCCH_Message" of type UL_DCCH_Message end "aM_message" of type CHOICE end "car_PhyChReconfCmpl" of type RLC_AM_DATA_IND CancelTimer:TSP1: [4] t_WaitMS [13500] 13500 ms Receive event:TSP1: [4] AM ? RLC_AM_DATA_IND = PDU (view PDU) Preliminary verdict:TSP1: [4] (PASS) Attach:[9] Exit Test Step ts_RRC_ReceivePhyChReconfCmpl
Attach:[16] Exit Test Step ts_PhyChannelReconfig_NoTFCI
Assignment:[17] tcv_Tolerance := 500 StartTimer:[18] t_WaitMS [13500] 5500 ms 00:01:55.660 - Primitive: RLC_UM_DATA_IND: measurementReport 00:01:55.660 - Primitive: RLC_UM_DATA_IND begin "car_MeasurementReportUM" of type RLC_UM_DATA_IND (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "integrityResult" of type IntegrityResult (CHOICE) [UNIVERSAL 31] matching [integrityUsed: i_pass] against * end "integrityResult" of type IntegrityResult begin "uM_message" of type CHOICE [UNIVERSAL 31] begin "uL_DCCH_Message" of type UL_DCCH_Message (SEQUENCE) [UNIVERSAL 16] begin "integrityCheckInfo" of type IntegrityCheckInfo (SEQUENCE) [UNIVERSAL 16] matching { messageAuthenticationCode: '10001100010111011100000101000001'B , rrc_MessageSequenceNumber: 1 } against * end "integrityCheckInfo" of type IntegrityCheckInfo begin "message" of type UL_DCCH_MessageType (CHOICE) [UNIVERSAL 31] begin "measurementReport" of type MeasurementReport (SEQUENCE) [UNIVERSAL 16] begin "measurementIdentity" of type MeasurementIdentity (INTEGER) [UNIVERSAL 2] matching 4 against 4 end "measurementIdentity" of type MeasurementIdentity begin "eventResults" of type EventResults (CHOICE) [UNIVERSAL 31] begin "interFreqEventResults" of type InterFreqEventResults (SEQUENCE) [UNIVERSAL 16] begin "eventID" of type EventIDInterFreq (ENUMERATED) [UNIVERSAL 10] matching e2e against e2e end "eventID" of type EventIDInterFreq begin "interFreqCellList" of type InterFreqCellList (SEQUENCEOF) [UNIVERSAL 28] begin InterFreqCell (SEQUENCE) [UNIVERSAL 16] begin "frequencyInfo" of type FrequencyInfo (SEQUENCE) [UNIVERSAL 16] begin "modeSpecificInfo" of type CHOICE [UNIVERSAL 31] begin "fdd" of type FrequencyInfoFDD (SEQUENCE) [UNIVERSAL 16] begin "uarfcn_DL" of type UARFCN (INTEGER) [UNIVERSAL 2] matching 10837 against 10837 end "uarfcn_DL" of type UARFCN end "fdd" of type FrequencyInfoFDD end "modeSpecificInfo" of type CHOICE end "frequencyInfo" of type FrequencyInfo begin "nonFreqRelatedEventResults" of type CellMeasurementEventResults (CHOICE) [UNIVERSAL 31] begin "fdd" of type SEQUENCEOF [UNIVERSAL 28] begin PrimaryCPICH_Info (SEQUENCE) [UNIVERSAL 16] begin "primaryScramblingCode" of type PrimaryScramblingCode (INTEGER) [UNIVERSAL 2] matching 250 against 250 end "primaryScramblingCode" of type PrimaryScramblingCode end PrimaryCPICH_Info end "fdd" of type SEQUENCEOF end "nonFreqRelatedEventResults" of type CellMeasurementEventResults end InterFreqCell end "interFreqCellList" of type InterFreqCellList end "interFreqEventResults" of type InterFreqEventResults end "eventResults" of type EventResults end "measurementReport" of type MeasurementReport end "message" of type UL_DCCH_MessageType end "uL_DCCH_Message" of type UL_DCCH_Message end "uM_message" of type CHOICE end "car_MeasurementReportUM" of type RLC_UM_DATA_IND Receive event:TBP1: [20] UM ? RLC_UM_DATA_IND = PDU (view PDU) Preliminary verdict:TBP1: [20] (PASS) CancelTimer:[21] t_WaitMS [13500] 5500 ms Assignment:[22] attenuationLevel := 0 Attach:[23] Enter Test Step ts_SetAttenuationLevel( 3 )
| Assignment:[11] attenuationLevel := 0 Attach:[12] Enter Test Step ts_SetAttenuationLevel::lt_SetAttLev( 3 )
| 00:01:55.660 - Primitive: CPHY_Cell_TxPower_Modify_REQ Send event:[26] CPHY ! CPHY_Cell_TxPower_Modify_REQ = PDU: { cellId: 3 , dLTxAttenuationLevel: 0 } 00:01:55.720 - Primitive: CPHY_Cell_TxPower_Modify_CNF begin "ca_CellTxPowerModiCnf" of type CPHY_Cell_TxPower_Modify_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER end "ca_CellTxPowerModiCnf" of type CPHY_Cell_TxPower_Modify_CNF Receive event:[27] CPHY ? CPHY_Cell_TxPower_Modify_CNF = PDU: { cellId: 3 } Attach:[12] Exit Test Step ts_SetAttenuationLevel::lt_SetAttLev
Attach:[23] Exit Test Step ts_SetAttenuationLevel
StartTimer:[24] t_WaitMS [13500] 10000 ms Timed out Timer:t_WaitMS TimeOut:TBP2: [26] t_WaitMS [13500] 10000 ms Preliminary verdict:TBP2: [26] (PASS) Assignment:[27] attenuationLevel := 25 Attach:[28] Enter Test Step ts_SetAttenuationLevel( 0 )
| Assignment:[2] attenuationLevel := 25 Attach:[3] Enter Test Step ts_SetAttenuationLevel::lt_SetAttLev( 0 )
| 00:02:05.740 - Primitive: CPHY_Cell_TxPower_Modify_REQ Send event:[26] CPHY ! CPHY_Cell_TxPower_Modify_REQ = PDU: { cellId: 0 , dLTxAttenuationLevel: 25 } 00:02:05.850 - Primitive: CPHY_Cell_TxPower_Modify_CNF begin "ca_CellTxPowerModiCnf" of type CPHY_Cell_TxPower_Modify_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER end "ca_CellTxPowerModiCnf" of type CPHY_Cell_TxPower_Modify_CNF Receive event:[27] CPHY ? CPHY_Cell_TxPower_Modify_CNF = PDU: { cellId: 0 } Attach:[3] Exit Test Step ts_SetAttenuationLevel::lt_SetAttLev
Attach:[28] Exit Test Step ts_SetAttenuationLevel
Assignment:[29] tcv_Tolerance := 500 StartTimer:[30] t_WaitMS [13500] 4500 ms Timed out Timer:t_WaitMS TimeOut:[31] t_WaitMS [13500] 4500 ms 00:02:11.410 - Primitive: RLC_UM_DATA_IND: measurementReport 00:02:11.410 - Primitive: RLC_UM_DATA_IND begin "car_MeasurementReportUM" of type RLC_UM_DATA_IND (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "integrityResult" of type IntegrityResult (CHOICE) [UNIVERSAL 31] matching [integrityUsed: i_pass] against * end "integrityResult" of type IntegrityResult begin "uM_message" of type CHOICE [UNIVERSAL 31] begin "uL_DCCH_Message" of type UL_DCCH_Message (SEQUENCE) [UNIVERSAL 16] begin "integrityCheckInfo" of type IntegrityCheckInfo (SEQUENCE) [UNIVERSAL 16] matching { messageAuthenticationCode: '01101111000101011100010000110101'B , rrc_MessageSequenceNumber: 2 } against * end "integrityCheckInfo" of type IntegrityCheckInfo begin "message" of type UL_DCCH_MessageType (CHOICE) [UNIVERSAL 31] begin "measurementReport" of type MeasurementReport (SEQUENCE) [UNIVERSAL 16] begin "measurementIdentity" of type MeasurementIdentity (INTEGER) [UNIVERSAL 2] matching 4 against 4 end "measurementIdentity" of type MeasurementIdentity begin "measuredResults" of type MeasuredResults (CHOICE) [UNIVERSAL 31] begin "interFreqMeasuredResultsList" of type InterFreqMeasuredResultsList (SEQUENCEOF) [UNIVERSAL 28] begin InterFreqMeasuredResults (SEQUENCE) [UNIVERSAL 16] begin "frequencyInfo" of type FrequencyInfo (SEQUENCE) [UNIVERSAL 16] begin "modeSpecificInfo" of type CHOICE [UNIVERSAL 31] begin "fdd" of type FrequencyInfoFDD (SEQUENCE) [UNIVERSAL 16] begin "uarfcn_DL" of type UARFCN (INTEGER) [UNIVERSAL 2] matching 10837 against 10837 end "uarfcn_DL" of type UARFCN end "fdd" of type FrequencyInfoFDD end "modeSpecificInfo" of type CHOICE end "frequencyInfo" of type FrequencyInfo begin "interFreqCellMeasuredResultsList" of type InterFreqCellMeasuredResultsList (SEQUENCEOF) [UNIVERSAL 28] begin CellMeasuredResults (SEQUENCE) [UNIVERSAL 16] begin "modeSpecificInfo" of type CHOICE [UNIVERSAL 31] begin "fdd" of type SEQUENCE [UNIVERSAL 16] begin "primaryCPICH_Info" of type PrimaryCPICH_Info (SEQUENCE) [UNIVERSAL 16] begin "primaryScramblingCode" of type PrimaryScramblingCode (INTEGER) [UNIVERSAL 2] matching 250 against 250 end "primaryScramblingCode" of type PrimaryScramblingCode end "primaryCPICH_Info" of type PrimaryCPICH_Info begin "cpich_RSCP" of type CPICH_RSCP (INTEGER) [UNIVERSAL 2] matching 55 against ? end "cpich_RSCP" of type CPICH_RSCP end "fdd" of type SEQUENCE end "modeSpecificInfo" of type CHOICE end CellMeasuredResults end "interFreqCellMeasuredResultsList" of type InterFreqCellMeasuredResultsList end InterFreqMeasuredResults end "interFreqMeasuredResultsList" of type InterFreqMeasuredResultsList end "measuredResults" of type MeasuredResults begin "eventResults" of type EventResults (CHOICE) [UNIVERSAL 31] begin "interFreqEventResults" of type InterFreqEventResults (SEQUENCE) [UNIVERSAL 16] begin "eventID" of type EventIDInterFreq (ENUMERATED) [UNIVERSAL 10] matching e2b against e2b end "eventID" of type EventIDInterFreq begin "interFreqCellList" of type InterFreqCellList (SEQUENCEOF) [UNIVERSAL 28] begin InterFreqCell (SEQUENCE) [UNIVERSAL 16] begin "frequencyInfo" of type FrequencyInfo (SEQUENCE) [UNIVERSAL 16] begin "modeSpecificInfo" of type CHOICE [UNIVERSAL 31] begin "fdd" of type FrequencyInfoFDD (SEQUENCE) [UNIVERSAL 16] begin "uarfcn_DL" of type UARFCN (INTEGER) [UNIVERSAL 2] matching 10837 against 10837 end "uarfcn_DL" of type UARFCN end "fdd" of type FrequencyInfoFDD end "modeSpecificInfo" of type CHOICE end "frequencyInfo" of type FrequencyInfo begin "nonFreqRelatedEventResults" of type CellMeasurementEventResults (CHOICE) [UNIVERSAL 31] begin "fdd" of type SEQUENCEOF [UNIVERSAL 28] begin PrimaryCPICH_Info (SEQUENCE) [UNIVERSAL 16] begin "primaryScramblingCode" of type PrimaryScramblingCode (INTEGER) [UNIVERSAL 2] matching 250 against 250 end "primaryScramblingCode" of type PrimaryScramblingCode end PrimaryCPICH_Info end "fdd" of type SEQUENCEOF end "nonFreqRelatedEventResults" of type CellMeasurementEventResults end InterFreqCell end "interFreqCellList" of type InterFreqCellList end "interFreqEventResults" of type InterFreqEventResults end "eventResults" of type EventResults end "measurementReport" of type MeasurementReport end "message" of type UL_DCCH_MessageType end "uL_DCCH_Message" of type UL_DCCH_Message end "uM_message" of type CHOICE end "car_MeasurementReportUM" of type RLC_UM_DATA_IND Receive event:TBP3: [32] UM ? RLC_UM_DATA_IND = PDU (view PDU) Preliminary verdict:TBP3: [32] (PASS) Attach:[33] Enter Test Step ts_C3_CheckCellDCH( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[2] Enter Test Step ts_RRC_Delay( 1000 )
| StartTimer:[1] t_Dly [5000] 1000 ms Timed out Timer:t_Dly TimeOut:[2] t_Dly [5000] 1000 ms Attach:[2] Exit Test Step ts_RRC_Delay
Attach:[3] Enter Test Step ts_C3_CheckCellDCH_NoNAS( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[2] Enter Test Step ts_C3_CheckCellDCH_NoNAS::lt_Send_RRC_ConnectionRelease( 0 )
| Assignment:[10] tcv_N308 := 1 Assignment:[10] tcv_K := 1 00:02:12.430 - Primitive: RLC_UM_DATA_REQ 00:02:12.430 - Primitive: RLC_UM_DATA_REQ: rrcConnectionRelease Send event:[11] UM ! RLC_UM_DATA_REQ = PDU (view PDU) StartTimer:[11] t_WaitMS [13500] 13500 ms 00:02:12.850 - Primitive: RLC_UM_DATA_IND: rrcConnectionReleaseComplete 00:02:12.850 - Primitive: RLC_UM_DATA_IND begin "car_RRC_ConnRelCmplUM" of type RLC_UM_DATA_IND (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "integrityResult" of type IntegrityResult (CHOICE) [UNIVERSAL 31] matching [integrityUsed: i_pass] against * end "integrityResult" of type IntegrityResult begin "uM_message" of type CHOICE [UNIVERSAL 31] begin "uL_DCCH_Message" of type UL_DCCH_Message (SEQUENCE) [UNIVERSAL 16] begin "integrityCheckInfo" of type IntegrityCheckInfo (SEQUENCE) [UNIVERSAL 16] matching { messageAuthenticationCode: '01100011110001101001000110000100'B , rrc_MessageSequenceNumber: 3 } against * end "integrityCheckInfo" of type IntegrityCheckInfo begin "message" of type UL_DCCH_MessageType (CHOICE) [UNIVERSAL 31] begin "rrcConnectionReleaseComplete" of type RRCConnectionReleaseComplete (SEQUENCE) [UNIVERSAL 16] begin "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier (INTEGER) [UNIVERSAL 2] matching 0 against 0 end "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier end "rrcConnectionReleaseComplete" of type RRCConnectionReleaseComplete end "message" of type UL_DCCH_MessageType end "uL_DCCH_Message" of type UL_DCCH_Message end "uM_message" of type CHOICE end "car_RRC_ConnRelCmplUM" of type RLC_UM_DATA_IND CancelTimer:TSP1: [12] t_WaitMS [13500] 13500 ms Receive event:TSP1: [12] UM ? RLC_UM_DATA_IND = PDU (view PDU) Preliminary verdict:TSP1: [12] (PASS) Attach:[13] Enter Test Step ts_C3_CheckCellDCH_NoNAS::lt_RptRcvConnRel( 0 )
| StartTimer:[15] t_Dly [5000] 5000 ms 00:02:13.020 - Primitive: RLC_UM_DATA_IND: rrcConnectionReleaseComplete 00:02:13.020 - Primitive: RLC_UM_DATA_IND begin "car_RRC_ConnRelCmplUM" of type RLC_UM_DATA_IND (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo begin "integrityResult" of type IntegrityResult (CHOICE) [UNIVERSAL 31] matching [integrityUsed: i_pass] against * end "integrityResult" of type IntegrityResult begin "uM_message" of type CHOICE [UNIVERSAL 31] begin "uL_DCCH_Message" of type UL_DCCH_Message (SEQUENCE) [UNIVERSAL 16] begin "integrityCheckInfo" of type IntegrityCheckInfo (SEQUENCE) [UNIVERSAL 16] matching { messageAuthenticationCode: '00101011001011111001011000101110'B , rrc_MessageSequenceNumber: 4 } against * end "integrityCheckInfo" of type IntegrityCheckInfo begin "message" of type UL_DCCH_MessageType (CHOICE) [UNIVERSAL 31] begin "rrcConnectionReleaseComplete" of type RRCConnectionReleaseComplete (SEQUENCE) [UNIVERSAL 16] begin "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier (INTEGER) [UNIVERSAL 2] matching 0 against 0 end "rrc_TransactionIdentifier" of type RRC_TransactionIdentifier end "rrcConnectionReleaseComplete" of type RRCConnectionReleaseComplete end "message" of type UL_DCCH_MessageType end "uL_DCCH_Message" of type UL_DCCH_Message end "uM_message" of type CHOICE end "car_RRC_ConnRelCmplUM" of type RLC_UM_DATA_IND Assignment:TSP2: [18] tcv_K := 2 CancelTimer:TSP2: [18] t_Dly [5000] 5000 ms Receive event:TSP2: [18] UM ? RLC_UM_DATA_IND = PDU (view PDU) Preliminary verdict:TSP2: [18] (PASS) Attach:[13] Exit Test Step ts_C3_CheckCellDCH_NoNAS::lt_RptRcvConnRel
Attach:[2] Exit Test Step ts_C3_CheckCellDCH_NoNAS::lt_Send_RRC_ConnectionRelease
Attach:[3] Enter Test Step ts_C3_CheckCellDCH_NoNAS::lt_RestartCRLC_ForNextConnection( 0 )
| Attach:[7] Enter Test Step ts_SS_ReconfigRAB_ToSRB( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[2] Enter Test Step ts_SS_RelDPCH( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[11] Enter Test Step ts_SS_RelDPCH::lt_RelSRB1_4( 0 )
| Attach:[97] Enter Test Step ts_CRLC_Rel( -1 )
| 00:02:13.020 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:02:13.220 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 1 ]} Attach:[97] Exit Test Step ts_CRLC_Rel
Attach:[98] Enter Test Step ts_CRLC_Rel( -1 )
| 00:02:13.220 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:02:13.270 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 2 ]} Attach:[98] Exit Test Step ts_CRLC_Rel
Attach:[99] Enter Test Step ts_CRLC_Rel( -1 )
| 00:02:13.270 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:02:13.380 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 3 ]} Attach:[99] Exit Test Step ts_CRLC_Rel
Attach:[100] Enter Test Step ts_CRLC_Rel( -1 )
| 00:02:13.380 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:02:13.490 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 4 ]} Attach:[100] Exit Test Step ts_CRLC_Rel
Attach:[11] Exit Test Step ts_SS_RelDPCH::lt_RelSRB1_4
Attach:[12] Enter Test Step ts_CRLC_Rel( -1 )
| 00:02:13.490 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:02:13.520 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 10 against 10 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 10 ]} Attach:[12] Exit Test Step ts_CRLC_Rel
Attach:[13] Enter Test Step ts_CRLC_Rel( -1 )
| 00:02:13.520 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:02:13.690 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 11 against 11 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 11 ]} Attach:[13] Exit Test Step ts_CRLC_Rel
Attach:[14] Enter Test Step ts_CRLC_Rel( -1 )
| 00:02:13.690 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:02:13.860 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 12 against 12 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 12 ]} Attach:[14] Exit Test Step ts_CRLC_Rel
Attach:[15] Enter Test Step ts_CMAC_Rel( -1 )
| 00:02:13.860 - Primitive: CMAC_Config_REQ Send event:[1] CMAC ! CMAC_Config_REQ = PDU (view PDU) 00:02:13.910 - Primitive: CMAC_Config_CNF begin "ca_CMAC_CfgCnf" of type CMAC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 26 against 26 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_CfgCnf" of type CMAC_Config_CNF Receive event:[2] CMAC ? CMAC_Config_CNF = PDU: { cellId: -1 , routingInfo: [physicalChannelIdentity: 26 ]} Attach:[15] Exit Test Step ts_CMAC_Rel
Attach:[16] Enter Test Step ts_CMAC_Rel( -1 )
| 00:02:13.910 - Primitive: CMAC_Config_REQ Send event:[1] CMAC ! CMAC_Config_REQ = PDU (view PDU) 00:02:13.940 - Primitive: CMAC_Config_CNF begin "ca_CMAC_CfgCnf" of type CMAC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 20 against 20 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_CfgCnf" of type CMAC_Config_CNF Receive event:[2] CMAC ? CMAC_Config_CNF = PDU: { cellId: -1 , routingInfo: [physicalChannelIdentity: 20 ]} Attach:[16] Exit Test Step ts_CMAC_Rel
Attach:[17] Enter Test Step ts_CPHY_TrChRelDCH_NoSHO( 0 )
| 00:02:13.940 - Primitive: CPHY_TrCH_Release_REQ Send event:[1] CPHY ! CPHY_TrCH_Release_REQ = PDU (view PDU) 00:02:13.970 - Primitive: CPHY_TrCH_Release_CNF begin "ca_PHY_RelCnf" of type CPHY_TrCH_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 26 against 26 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_PHY_RelCnf" of type CPHY_TrCH_Release_CNF Receive event:[2] CPHY ? CPHY_TrCH_Release_CNF = PDU (view PDU) Attach:[17] Exit Test Step ts_CPHY_TrChRelDCH_NoSHO
Attach:[18] Enter Test Step ts_CPHY_TrChRelDCH_NoSHO( 0 )
| 00:02:13.970 - Primitive: CPHY_TrCH_Release_REQ Send event:[1] CPHY ! CPHY_TrCH_Release_REQ = PDU (view PDU) 00:02:14.000 - Primitive: CPHY_TrCH_Release_CNF begin "ca_PHY_RelCnf" of type CPHY_TrCH_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 20 against 20 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_PHY_RelCnf" of type CPHY_TrCH_Release_CNF Receive event:[2] CPHY ? CPHY_TrCH_Release_CNF = PDU (view PDU) Attach:[18] Exit Test Step ts_CPHY_TrChRelDCH_NoSHO
Attach:[19] Enter Test Step ts_SS_StopRL( 0 )
| 00:02:14.000 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 26 ]} 00:02:14.040 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 26 against 26 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 26 ]} Attach:[19] Exit Test Step ts_SS_StopRL
Attach:[20] Enter Test Step ts_SS_StopRL( 0 )
| 00:02:14.040 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 20 ]} 00:02:14.070 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 20 against 20 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 20 ]} Attach:[20] Exit Test Step ts_SS_StopRL
Attach:[2] Exit Test Step ts_SS_RelDPCH
Attach:[3] Enter Test Step ts_SS_1DCH_DCCH_Cfg( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Assignment:[3] tcv_TGCFN := 0 00:02:14.070 - Primitive: CPHY_RL_Setup_REQ Send event:[4] CPHY ! CPHY_RL_Setup_REQ = PDU (view PDU) 00:02:14.130 - Primitive: CPHY_RL_Setup_CNF begin "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 26 against 26 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF Receive event:[5] CPHY ? CPHY_RL_Setup_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 26 ]} 00:02:14.130 - Primitive: CPHY_TrCH_Config_REQ Send event:[6] CPHY ! CPHY_TrCH_Config_REQ = PDU (view PDU) 00:02:14.160 - Primitive: CPHY_TrCH_Config_CNF begin "ca_TrChCfgCnf" of type CPHY_TrCH_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 26 against 26 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_TrChCfgCnf" of type CPHY_TrCH_Config_CNF Receive event:[7] CPHY ? CPHY_TrCH_Config_CNF = PDU (view PDU) 00:02:14.160 - Primitive: CMAC_Config_REQ Send event:[8] CMAC ! CMAC_Config_REQ = PDU (view PDU) 00:02:14.190 - Primitive: CMAC_Config_CNF begin "ca_CMAC_CfgCnf" of type CMAC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 26 against 26 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_CfgCnf" of type CMAC_Config_CNF Receive event:[9] CMAC ? CMAC_Config_CNF = PDU: { cellId: -1 , routingInfo: [physicalChannelIdentity: 26 ]} 00:02:14.190 - Primitive: CPHY_RL_Setup_REQ Send event:[10] CPHY ! CPHY_RL_Setup_REQ = PDU (view PDU) 00:02:14.210 - Primitive: CPHY_RL_Setup_CNF begin "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 20 against 20 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_SetupCnf" of type CPHY_RL_Setup_CNF Receive event:[11] CPHY ? CPHY_RL_Setup_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 20 ]} 00:02:14.210 - Primitive: CPHY_TrCH_Config_REQ Send event:[12] CPHY ! CPHY_TrCH_Config_REQ = PDU (view PDU) 00:02:14.410 - Primitive: CPHY_TrCH_Config_CNF begin "ca_TrChCfgCnf" of type CPHY_TrCH_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 20 against 20 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_TrChCfgCnf" of type CPHY_TrCH_Config_CNF Receive event:[13] CPHY ? CPHY_TrCH_Config_CNF = PDU (view PDU) 00:02:14.410 - Primitive: CMAC_Config_REQ Send event:[14] CMAC ! CMAC_Config_REQ = PDU (view PDU) 00:02:14.440 - Primitive: CMAC_Config_CNF begin "ca_CMAC_CfgCnf" of type CMAC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 20 against 20 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_CfgCnf" of type CMAC_Config_CNF Receive event:[15] CMAC ? CMAC_Config_CNF = PDU: { cellId: -1 , routingInfo: [physicalChannelIdentity: 20 ]} Attach:[3] Exit Test Step ts_SS_1DCH_DCCH_Cfg
Attach:[4] Enter Test Step ts_SS_RB1_ToRB4_Cfg( )
| 00:02:14.440 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:02:14.490 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 1 ]} 00:02:14.490 - Primitive: CRLC_Config_REQ Send event:[3] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:02:14.570 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[4] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 2 ]} 00:02:14.570 - Primitive: CRLC_Config_REQ Send event:[5] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:02:14.640 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[6] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 3 ]} 00:02:14.640 - Primitive: CRLC_Config_REQ Send event:[7] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:02:14.790 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[8] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 4 ]} Attach:[4] Exit Test Step ts_SS_RB1_ToRB4_Cfg
Attach:[7] Exit Test Step ts_SS_ReconfigRAB_ToSRB
Attach:[8] Enter Test Step ts_SetCellCfg( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Assignment:[2] cellConfig := cell_DCH_StandAloneSRB_NoConn Attach:[3] Enter Test Step ts_SaveCellInfo( 0 )
| Assignment:[2] tcv_CellInfoA := (view Assignment) Attach:[3] Exit Test Step ts_SaveCellInfo
Attach:[8] Exit Test Step ts_SetCellCfg
Attach:[3] Exit Test Step ts_C3_CheckCellDCH_NoNAS::lt_RestartCRLC_ForNextConnection
Attach:[3] Exit Test Step ts_C3_CheckCellDCH_NoNAS
Attach:[33] Exit Test Step ts_C3_CheckCellDCH
Assignment:TBE: [34] tcv_TestBody := GcFALSE Preliminary verdict:TBE: [34] (PASS) Attach:[10] Exit Test Step tc_8_4_1_25::lt_TestBody
Attach:[11] Enter Test Step po_ConnectionAndSS_Rels( )
| Attach:[1] Enter Test Step po_ConnectionAndSS_Rels::lt_ReleaseCell( 0 )
| Attach:[9] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[9] Exit Test Step ts_SetTmpCellInfo
Attach:[11] Enter Test Step po_ConnectionAndSS_Rel( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[3] Enter Test Step po_ConnectionAndSS_Rel::lt_Send_RRC_ConnectionRelease( 0 )
| Attach:[3] Exit Test Step po_ConnectionAndSS_Rel::lt_Send_RRC_ConnectionRelease
Attach:[4] Enter Test Step ts_SS_Rel( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[3] Enter Test Step ts_SS_RelDPCH( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[3] Enter Test Step ts_SS_RelDPCH::lt_RelSRB1_4( 0 )
| Attach:[97] Enter Test Step ts_CRLC_Rel( -1 )
| 00:02:14.790 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:02:14.960 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 1 ]} Attach:[97] Exit Test Step ts_CRLC_Rel
Attach:[98] Enter Test Step ts_CRLC_Rel( -1 )
| 00:02:14.960 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:02:14.990 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 2 ]} Attach:[98] Exit Test Step ts_CRLC_Rel
Attach:[99] Enter Test Step ts_CRLC_Rel( -1 )
| 00:02:14.990 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:02:15.130 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 3 ]} Attach:[99] Exit Test Step ts_CRLC_Rel
Attach:[100] Enter Test Step ts_CRLC_Rel( -1 )
| 00:02:15.130 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:02:15.240 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: -1 , routingInfo: [rB_Identity: 4 ]} Attach:[100] Exit Test Step ts_CRLC_Rel
Attach:[3] Exit Test Step ts_SS_RelDPCH::lt_RelSRB1_4
Attach:[4] Enter Test Step ts_CMAC_Rel( -1 )
| 00:02:15.240 - Primitive: CMAC_Config_REQ Send event:[1] CMAC ! CMAC_Config_REQ = PDU (view PDU) 00:02:15.270 - Primitive: CMAC_Config_CNF begin "ca_CMAC_CfgCnf" of type CMAC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 26 against 26 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_CfgCnf" of type CMAC_Config_CNF Receive event:[2] CMAC ? CMAC_Config_CNF = PDU: { cellId: -1 , routingInfo: [physicalChannelIdentity: 26 ]} Attach:[4] Exit Test Step ts_CMAC_Rel
Attach:[5] Enter Test Step ts_CMAC_Rel( -1 )
| 00:02:15.270 - Primitive: CMAC_Config_REQ Send event:[1] CMAC ! CMAC_Config_REQ = PDU (view PDU) 00:02:15.300 - Primitive: CMAC_Config_CNF begin "ca_CMAC_CfgCnf" of type CMAC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 20 against 20 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_CfgCnf" of type CMAC_Config_CNF Receive event:[2] CMAC ? CMAC_Config_CNF = PDU: { cellId: -1 , routingInfo: [physicalChannelIdentity: 20 ]} Attach:[5] Exit Test Step ts_CMAC_Rel
Attach:[6] Enter Test Step ts_CPHY_TrChRelDCH_NoSHO( 0 )
| 00:02:15.300 - Primitive: CPHY_TrCH_Release_REQ Send event:[1] CPHY ! CPHY_TrCH_Release_REQ = PDU (view PDU) 00:02:15.440 - Primitive: CPHY_TrCH_Release_CNF begin "ca_PHY_RelCnf" of type CPHY_TrCH_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 26 against 26 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_PHY_RelCnf" of type CPHY_TrCH_Release_CNF Receive event:[2] CPHY ? CPHY_TrCH_Release_CNF = PDU (view PDU) Attach:[6] Exit Test Step ts_CPHY_TrChRelDCH_NoSHO
Attach:[7] Enter Test Step ts_CPHY_TrChRelDCH_NoSHO( 0 )
| 00:02:15.440 - Primitive: CPHY_TrCH_Release_REQ Send event:[1] CPHY ! CPHY_TrCH_Release_REQ = PDU (view PDU) 00:02:15.470 - Primitive: CPHY_TrCH_Release_CNF begin "ca_PHY_RelCnf" of type CPHY_TrCH_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 20 against 20 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_PHY_RelCnf" of type CPHY_TrCH_Release_CNF Receive event:[2] CPHY ? CPHY_TrCH_Release_CNF = PDU (view PDU) Attach:[7] Exit Test Step ts_CPHY_TrChRelDCH_NoSHO
Attach:[8] Enter Test Step ts_SS_StopRL( 0 )
| 00:02:15.470 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 26 ]} 00:02:15.500 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 26 against 26 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 26 ]} Attach:[8] Exit Test Step ts_SS_StopRL
Attach:[9] Enter Test Step ts_SS_StopRL( 0 )
| 00:02:15.500 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 20 ]} 00:02:15.540 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 20 against 20 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 20 ]} Attach:[9] Exit Test Step ts_SS_StopRL
Attach:[3] Exit Test Step ts_SS_RelDPCH
Attach:[4] Enter Test Step ts_SS_Rel::lt_ReleaseCommonCh( 0 )
| Attach:[328] Enter Test Step ts_CRLC_Rel( 0 )
| 00:02:15.540 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:02:15.600 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: 0 ]} Attach:[328] Exit Test Step ts_CRLC_Rel
Attach:[329] Enter Test Step ts_CMAC_Rel( 0 )
| 00:02:15.600 - Primitive: CMAC_Config_REQ Send event:[1] CMAC ! CMAC_Config_REQ = PDU (view PDU) 00:02:15.630 - Primitive: CMAC_Config_CNF begin "ca_CMAC_CfgCnf" of type CMAC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 8 against 8 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_CfgCnf" of type CMAC_Config_CNF Receive event:[2] CMAC ? CMAC_Config_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 8 ]} Attach:[329] Exit Test Step ts_CMAC_Rel
Attach:[330] Enter Test Step ts_CPHY_TrChRelNonDch( 0 )
| 00:02:15.630 - Primitive: CPHY_TrCH_Release_REQ Send event:[1] CPHY ! CPHY_TrCH_Release_REQ = PDU (view PDU) 00:02:15.660 - Primitive: CPHY_TrCH_Release_CNF begin "ca_PHY_RelCnf" of type CPHY_TrCH_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 8 against 8 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_PHY_RelCnf" of type CPHY_TrCH_Release_CNF Receive event:[2] CPHY ? CPHY_TrCH_Release_CNF = PDU (view PDU) Attach:[330] Exit Test Step ts_CPHY_TrChRelNonDch
Attach:[331] Enter Test Step ts_SS_StopRL( 0 )
| 00:02:15.660 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 7 ]} 00:02:15.690 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 7 against 7 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 7 ]} Attach:[331] Exit Test Step ts_SS_StopRL
Attach:[332] Enter Test Step ts_SS_StopRL( 0 )
| 00:02:15.690 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 8 ]} 00:02:15.720 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 8 against 8 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 8 ]} Attach:[332] Exit Test Step ts_SS_StopRL
Attach:[333] Enter Test Step ts_CRLC_Rel( 0 )
| 00:02:15.720 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:02:15.770 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -2 against -2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -2 ]} Attach:[333] Exit Test Step ts_CRLC_Rel
Attach:[334] Enter Test Step ts_CMAC_Rel( 0 )
| 00:02:15.770 - Primitive: CMAC_Config_REQ Send event:[1] CMAC ! CMAC_Config_REQ = PDU (view PDU) 00:02:15.800 - Primitive: CMAC_Config_CNF begin "ca_CMAC_CfgCnf" of type CMAC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 5 against 5 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_CfgCnf" of type CMAC_Config_CNF Receive event:[2] CMAC ? CMAC_Config_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 5 ]} Attach:[334] Exit Test Step ts_CMAC_Rel
Attach:[335] Enter Test Step ts_CPHY_TrChRelNonDch( 0 )
| 00:02:15.800 - Primitive: CPHY_TrCH_Release_REQ Send event:[1] CPHY ! CPHY_TrCH_Release_REQ = PDU (view PDU) 00:02:15.830 - Primitive: CPHY_TrCH_Release_CNF begin "ca_PHY_RelCnf" of type CPHY_TrCH_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 5 against 5 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_PHY_RelCnf" of type CPHY_TrCH_Release_CNF Receive event:[2] CPHY ? CPHY_TrCH_Release_CNF = PDU (view PDU) Attach:[335] Exit Test Step ts_CPHY_TrChRelNonDch
Attach:[336] Enter Test Step ts_SS_StopRL( 0 )
| 00:02:15.830 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 6 ]} 00:02:15.860 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 6 ]} Attach:[336] Exit Test Step ts_SS_StopRL
Attach:[337] Enter Test Step ts_SS_StopRL( 0 )
| 00:02:15.860 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 5 ]} 00:02:15.890 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 5 against 5 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 5 ]} Attach:[337] Exit Test Step ts_SS_StopRL
Attach:[4] Exit Test Step ts_SS_Rel::lt_ReleaseCommonCh
Attach:[5] Enter Test Step ts_SS_Rel::lt_Release_BCCH( 0 )
| Attach:[321] Enter Test Step ts_CRLC_Rel( 0 )
| 00:02:15.890 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:02:16.100 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: 0 , routingInfo: [rB_Identity: -1 ]} Attach:[321] Exit Test Step ts_CRLC_Rel
Attach:[322] Enter Test Step ts_CMAC_Rel( 0 )
| 00:02:16.100 - Primitive: CMAC_Config_REQ Send event:[1] CMAC ! CMAC_Config_REQ = PDU (view PDU) 00:02:16.130 - Primitive: CMAC_Config_CNF begin "ca_CMAC_CfgCnf" of type CMAC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_CfgCnf" of type CMAC_Config_CNF Receive event:[2] CMAC ? CMAC_Config_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 4 ]} Attach:[322] Exit Test Step ts_CMAC_Rel
Attach:[323] Enter Test Step ts_CPHY_TrChRelNonDch( 0 )
| 00:02:16.130 - Primitive: CPHY_TrCH_Release_REQ Send event:[1] CPHY ! CPHY_TrCH_Release_REQ = PDU (view PDU) 00:02:16.160 - Primitive: CPHY_TrCH_Release_CNF begin "ca_PHY_RelCnf" of type CPHY_TrCH_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_PHY_RelCnf" of type CPHY_TrCH_Release_CNF Receive event:[2] CPHY ? CPHY_TrCH_Release_CNF = PDU (view PDU) Attach:[323] Exit Test Step ts_CPHY_TrChRelNonDch
Attach:[324] Enter Test Step ts_SS_StopRL( 0 )
| 00:02:16.160 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 2 ]} 00:02:16.190 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 2 ]} Attach:[324] Exit Test Step ts_SS_StopRL
Attach:[325] Enter Test Step ts_SS_StopRL( 0 )
| 00:02:16.190 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 1 ]} 00:02:16.220 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 1 ]} Attach:[325] Exit Test Step ts_SS_StopRL
Attach:[326] Enter Test Step ts_SS_StopRL( 0 )
| 00:02:16.220 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 4 ]} 00:02:16.250 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 4 ]} Attach:[326] Exit Test Step ts_SS_StopRL
Attach:[327] Enter Test Step ts_SS_StopRL( 0 )
| 00:02:16.250 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 0 ]} 00:02:16.290 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 0 , routingInfo: [physicalChannelIdentity: 0 ]} Attach:[327] Exit Test Step ts_SS_StopRL
Attach:[5] Exit Test Step ts_SS_Rel::lt_Release_BCCH
Attach:[6] Enter Test Step ts_SetCellCfg( 0 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 0 )
| Assignment:[2] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Assignment:[2] cellConfig := cell_NotConfigured Attach:[3] Enter Test Step ts_SaveCellInfo( 0 )
| Assignment:[2] tcv_CellInfoA := (view Assignment) Attach:[3] Exit Test Step ts_SaveCellInfo
Attach:[6] Exit Test Step ts_SetCellCfg
Attach:[4] Exit Test Step ts_SS_Rel
Attach:[11] Exit Test Step po_ConnectionAndSS_Rel
Attach:[1] Exit Test Step po_ConnectionAndSS_Rels::lt_ReleaseCell
Attach:[2] Enter Test Step po_ConnectionAndSS_Rels::lt_ReleaseCell( 1 )
| Attach:[9] Enter Test Step ts_SetTmpCellInfo( 1 )
| Assignment:[4] tcv_TmpCellInfo := (view Assignment) Attach:[9] Exit Test Step ts_SetTmpCellInfo
Attach:[2] Exit Test Step po_ConnectionAndSS_Rels::lt_ReleaseCell
Attach:[3] Enter Test Step po_ConnectionAndSS_Rels::lt_ReleaseCell( 2 )
| Attach:[9] Enter Test Step ts_SetTmpCellInfo( 2 )
| Assignment:[6] tcv_TmpCellInfo := (view Assignment) Attach:[9] Exit Test Step ts_SetTmpCellInfo
Attach:[3] Exit Test Step po_ConnectionAndSS_Rels::lt_ReleaseCell
Attach:[4] Enter Test Step po_ConnectionAndSS_Rels::lt_ReleaseCell( 3 )
| Attach:[9] Enter Test Step ts_SetTmpCellInfo( 3 )
| Assignment:[8] tcv_TmpCellInfo := (view Assignment) Attach:[9] Exit Test Step ts_SetTmpCellInfo
Attach:[11] Enter Test Step po_ConnectionAndSS_Rel( 3 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 3 )
| Assignment:[8] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[3] Enter Test Step po_ConnectionAndSS_Rel::lt_Send_RRC_ConnectionRelease( 3 )
| Attach:[3] Exit Test Step po_ConnectionAndSS_Rel::lt_Send_RRC_ConnectionRelease
Attach:[4] Enter Test Step ts_SS_Rel( 3 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 3 )
| Assignment:[8] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Attach:[74] Enter Test Step ts_SS_Rel::lt_ReleaseCommonCh( 3 )
| Attach:[328] Enter Test Step ts_CRLC_Rel( 3 )
| 00:02:16.290 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:02:16.390 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: 0 ]} Attach:[328] Exit Test Step ts_CRLC_Rel
Attach:[329] Enter Test Step ts_CMAC_Rel( 3 )
| 00:02:16.390 - Primitive: CMAC_Config_REQ Send event:[1] CMAC ! CMAC_Config_REQ = PDU (view PDU) 00:02:16.430 - Primitive: CMAC_Config_CNF begin "ca_CMAC_CfgCnf" of type CMAC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 8 against 8 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_CfgCnf" of type CMAC_Config_CNF Receive event:[2] CMAC ? CMAC_Config_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 8 ]} Attach:[329] Exit Test Step ts_CMAC_Rel
Attach:[330] Enter Test Step ts_CPHY_TrChRelNonDch( 3 )
| 00:02:16.430 - Primitive: CPHY_TrCH_Release_REQ Send event:[1] CPHY ! CPHY_TrCH_Release_REQ = PDU (view PDU) 00:02:16.460 - Primitive: CPHY_TrCH_Release_CNF begin "ca_PHY_RelCnf" of type CPHY_TrCH_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 8 against 8 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_PHY_RelCnf" of type CPHY_TrCH_Release_CNF Receive event:[2] CPHY ? CPHY_TrCH_Release_CNF = PDU (view PDU) Attach:[330] Exit Test Step ts_CPHY_TrChRelNonDch
Attach:[331] Enter Test Step ts_SS_StopRL( 3 )
| 00:02:16.460 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 7 ]} 00:02:16.490 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 7 against 7 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 7 ]} Attach:[331] Exit Test Step ts_SS_StopRL
Attach:[332] Enter Test Step ts_SS_StopRL( 3 )
| 00:02:16.490 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 8 ]} 00:02:16.520 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 8 against 8 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 8 ]} Attach:[332] Exit Test Step ts_SS_StopRL
Attach:[333] Enter Test Step ts_CRLC_Rel( 3 )
| 00:02:16.520 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:02:16.570 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -2 against -2 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -2 ]} Attach:[333] Exit Test Step ts_CRLC_Rel
Attach:[334] Enter Test Step ts_CMAC_Rel( 3 )
| 00:02:16.570 - Primitive: CMAC_Config_REQ Send event:[1] CMAC ! CMAC_Config_REQ = PDU (view PDU) 00:02:16.580 - Primitive: CMAC_Config_CNF begin "ca_CMAC_CfgCnf" of type CMAC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 5 against 5 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_CfgCnf" of type CMAC_Config_CNF Receive event:[2] CMAC ? CMAC_Config_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 5 ]} Attach:[334] Exit Test Step ts_CMAC_Rel
Attach:[335] Enter Test Step ts_CPHY_TrChRelNonDch( 3 )
| 00:02:16.580 - Primitive: CPHY_TrCH_Release_REQ Send event:[1] CPHY ! CPHY_TrCH_Release_REQ = PDU (view PDU) 00:02:16.610 - Primitive: CPHY_TrCH_Release_CNF begin "ca_PHY_RelCnf" of type CPHY_TrCH_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 5 against 5 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_PHY_RelCnf" of type CPHY_TrCH_Release_CNF Receive event:[2] CPHY ? CPHY_TrCH_Release_CNF = PDU (view PDU) Attach:[335] Exit Test Step ts_CPHY_TrChRelNonDch
Attach:[336] Enter Test Step ts_SS_StopRL( 3 )
| 00:02:16.610 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 6 ]} 00:02:16.640 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 6 against 6 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 6 ]} Attach:[336] Exit Test Step ts_SS_StopRL
Attach:[337] Enter Test Step ts_SS_StopRL( 3 )
| 00:02:16.640 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 5 ]} 00:02:16.680 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 5 against 5 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 5 ]} Attach:[337] Exit Test Step ts_SS_StopRL
Attach:[74] Exit Test Step ts_SS_Rel::lt_ReleaseCommonCh
Attach:[75] Enter Test Step ts_SS_Rel::lt_Release_BCCH( 3 )
| Attach:[321] Enter Test Step ts_CRLC_Rel( 3 )
| 00:02:16.680 - Primitive: CRLC_Config_REQ Send event:[1] CRLC ! CRLC_Config_REQ = PDU (view PDU) 00:02:16.720 - Primitive: CRLC_Config_CNF begin "ca_CRLC_CfgCnf" of type CRLC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "rB_Identity" of type INTEGER [UNIVERSAL 2] matching -1 against -1 end "rB_Identity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CRLC_CfgCnf" of type CRLC_Config_CNF Receive event:[2] CRLC ? CRLC_Config_CNF = PDU: { cellId: 3 , routingInfo: [rB_Identity: -1 ]} Attach:[321] Exit Test Step ts_CRLC_Rel
Attach:[322] Enter Test Step ts_CMAC_Rel( 3 )
| 00:02:16.720 - Primitive: CMAC_Config_REQ Send event:[1] CMAC ! CMAC_Config_REQ = PDU (view PDU) 00:02:16.770 - Primitive: CMAC_Config_CNF begin "ca_CMAC_CfgCnf" of type CMAC_Config_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_CMAC_CfgCnf" of type CMAC_Config_CNF Receive event:[2] CMAC ? CMAC_Config_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 4 ]} Attach:[322] Exit Test Step ts_CMAC_Rel
Attach:[323] Enter Test Step ts_CPHY_TrChRelNonDch( 3 )
| 00:02:16.770 - Primitive: CPHY_TrCH_Release_REQ Send event:[1] CPHY ! CPHY_TrCH_Release_REQ = PDU (view PDU) 00:02:16.800 - Primitive: CPHY_TrCH_Release_CNF begin "ca_PHY_RelCnf" of type CPHY_TrCH_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_PHY_RelCnf" of type CPHY_TrCH_Release_CNF Receive event:[2] CPHY ? CPHY_TrCH_Release_CNF = PDU (view PDU) Attach:[323] Exit Test Step ts_CPHY_TrChRelNonDch
Attach:[324] Enter Test Step ts_SS_StopRL( 3 )
| 00:02:16.800 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 2 ]} 00:02:16.830 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 2 against 2 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 2 ]} Attach:[324] Exit Test Step ts_SS_StopRL
Attach:[325] Enter Test Step ts_SS_StopRL( 3 )
| 00:02:16.830 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 1 ]} 00:02:16.860 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 1 against 1 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 1 ]} Attach:[325] Exit Test Step ts_SS_StopRL
Attach:[326] Enter Test Step ts_SS_StopRL( 3 )
| 00:02:16.860 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 4 ]} 00:02:16.890 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 4 against 4 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 4 ]} Attach:[326] Exit Test Step ts_SS_StopRL
Attach:[327] Enter Test Step ts_SS_StopRL( 3 )
| 00:02:16.890 - Primitive: CPHY_RL_Release_REQ Send event:[1] CPHY ! CPHY_RL_Release_REQ = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 0 ]} 00:02:16.930 - Primitive: CPHY_RL_Release_CNF begin "ca_RL_RelCnf" of type CPHY_RL_Release_CNF (SEQUENCE) [UNIVERSAL 16] begin "cellId" of type INTEGER [UNIVERSAL 2] matching 3 against 3 end "cellId" of type INTEGER begin "routingInfo" of type RoutingInfo (CHOICE) [UNIVERSAL 31] begin "physicalChannelIdentity" of type INTEGER [UNIVERSAL 2] matching 0 against 0 end "physicalChannelIdentity" of type INTEGER end "routingInfo" of type RoutingInfo end "ca_RL_RelCnf" of type CPHY_RL_Release_CNF Receive event:[2] CPHY ? CPHY_RL_Release_CNF = PDU: { cellId: 3 , routingInfo: [physicalChannelIdentity: 0 ]} Attach:[327] Exit Test Step ts_SS_StopRL
Attach:[75] Exit Test Step ts_SS_Rel::lt_Release_BCCH
Attach:[76] Enter Test Step ts_SetCellCfg( 3 )
| Attach:[1] Enter Test Step ts_SetTmpCellInfo( 3 )
| Assignment:[8] tcv_TmpCellInfo := (view Assignment) Attach:[1] Exit Test Step ts_SetTmpCellInfo
Assignment:[2] cellConfig := cell_NotConfigured Attach:[3] Enter Test Step ts_SaveCellInfo( 3 )
| Assignment:[8] tcv_CellInfoD := (view Assignment) Attach:[3] Exit Test Step ts_SaveCellInfo
Attach:[76] Exit Test Step ts_SetCellCfg
Attach:[4] Exit Test Step ts_SS_Rel
Attach:[11] Exit Test Step po_ConnectionAndSS_Rel
Attach:[4] Exit Test Step po_ConnectionAndSS_Rels::lt_ReleaseCell
Attach:[5] Enter Test Step po_ConnectionAndSS_Rels::lt_ReleaseCell( 4 )
| Attach:[9] Enter Test Step ts_SetTmpCellInfo( 4 )
| Assignment:[10] tcv_TmpCellInfo := (view Assignment) Attach:[9] Exit Test Step ts_SetTmpCellInfo
Attach:[5] Exit Test Step po_ConnectionAndSS_Rels::lt_ReleaseCell
Attach:[6] Enter Test Step po_ConnectionAndSS_Rels::lt_ReleaseCell( 5 )
| Attach:[9] Enter Test Step ts_SetTmpCellInfo( 5 )
| Assignment:[12] tcv_TmpCellInfo := (view Assignment) Attach:[9] Exit Test Step ts_SetTmpCellInfo
Attach:[6] Exit Test Step po_ConnectionAndSS_Rels::lt_ReleaseCell
Attach:[7] Enter Test Step po_ConnectionAndSS_Rels::lt_ReleaseCell( 6 )
| Attach:[9] Enter Test Step ts_SetTmpCellInfo( 6 )
| Assignment:[14] tcv_TmpCellInfo := (view Assignment) Attach:[9] Exit Test Step ts_SetTmpCellInfo
Attach:[7] Exit Test Step po_ConnectionAndSS_Rels::lt_ReleaseCell
Attach:[8] Enter Test Step po_ConnectionAndSS_Rels::lt_ReleaseCell( 7 )
| Attach:[9] Enter Test Step ts_SetTmpCellInfo( 7 )
| Assignment:[16] tcv_TmpCellInfo := (view Assignment) Attach:[9] Exit Test Step ts_SetTmpCellInfo
Attach:[8] Exit Test Step po_ConnectionAndSS_Rels::lt_ReleaseCell
Attach:[11] Exit Test Step po_ConnectionAndSS_Rels
CancelTimer:[(implicit)] t_Guard [300] 300 s