| RRC_wk26-tc_8_4_1_25ps_2004-07-12_13.09.01

#### MMI_CmdReq

RRC |  | LLA | @ 00:00:05.160

| Message Details:
| MMI_CmdReq:
cmd (IA5String): | Please switch off the UE

#### CPHY INI REQ

RRC |  | PHY | @ 00:00:06.200

| Message Details:
RAN Protocol Specification: | 2002-03 R99
| Physical Layer Parameters:
Timing: | Output
Clock: | Output
ISDN Board: | ISDN
| Layer 2 Parameters:
TM bit mode: | enabled

#### CPHY INI CNF

PHY |  | RRC | @ 00:00:06.990

| Message Details:
CAPI Version: | 2.10E1_CIPHER
Release: | MX785201A_2_10E1_INTA_A_CIPHER
| MD8480 pool:
| BTS Group 1:
Software: | V5.00h_FH_Cipher
FPGA: | V5.00
| Hardware Slots:
0: | TIMING GENERATOR
1: | TX BASEBAND
2: | TX BASEBAND
3: | TX BASEBAND
4: | FRAME CODER
5: | FRAME CODER
6: | RX BASEBAND
9: | ISDN V5.00
10: | RX BASEBAND
12: | FRAME DECODER
13: | VOICE CODEC
14: | TDMA V5.00b_FH
15: | CPU
| Options:
0: | Tx Diversity
1: | Compressed Mode
2: | Integrity & Ciphering
3: | V5.00
4: | CSD
| Physical Layer Parameters:
Timing: | Output
Clock: | Output
ISDN Board: | ISDN

#### MMI_CmdCnf

LLA |  | RRC | @ 00:00:07.960

| Message Details:
| MMI_CmdCnf:
result: | true
resultString (IA5String): | Omit

#### CPHY_Ini_REQ

RRC |  | LLA | @ 00:00:07.960

| Message Details:
CPHY_Ini_REQ: | defaultRadioEnvironment

#### CPHY BTS Configuration REQ

LLA |  | PHY | @ 00:00:08.670

| BTS unit: |  | 1:1
| CFN: |  | 108

| Message Details:
| Configuration Parameters:
Power Mode: | Normal Power Mode
RF Connector: | Main
Baseband Adder: | Off
LVDS: | Off
Timing: | 0
Delta Frequency: | 0
Delta Phase: | 0
| Downlink Parameters:
Frequency: | 2140000000
| Uplink Parameters:
Frequency: | 1950000000
| Tx Parameters:
Baseband Connector: | Analogue
Baseband Delay: | Not Used
| CCH Parameters:
Coder: | Tx Coder1 #1
Baseband: | Tx Baseband1
RF: | Tx RF #1
| DCH Parameters:
Coder: | Tx Coder1 #2
Baseband: | Tx Baseband1
RF: | Tx RF #1
| Rx Parameters:
Baseband Connector: | RF
RxMode: | Simultaneous PRACH/UL_DPCH
| CCH Parameters:
Coder: | Rx Decoder1 #1
Baseband: | Rx Baseband1
RF: | Rx RF #1
| DCH Parameters:
Coder: | Rx Decoder1 #2
Baseband: | Rx Baseband1
RF: | Rx RF #1

#### CPHY BTS Configuration REQ

LLA |  | PHY | @ 00:00:08.670

| BTS unit: |  | 1:2
| CFN: |  | 108

| Message Details:
| Configuration Parameters:
Power Mode: | Normal Power Mode
RF Connector: | Main
Baseband Adder: | On
LVDS: | Off
Timing: | 0
Delta Frequency: | 0
Delta Phase: | 0
| Downlink Parameters:
Frequency: | -2118567296
| Uplink Parameters:
Frequency: | 1977400000
| Tx Parameters:
Baseband Connector: | Analogue
Baseband Delay: | Not Used
| CCH Parameters:
Coder: | Tx Coder2 #1
Baseband: | Tx Baseband2
RF: | Tx RF #2
| DCH Parameters:
Coder: | Tx Coder1 #2
Baseband: | Tx Baseband2
RF: | Tx RF #2
| Rx Parameters:
Baseband Connector: | RF
RxMode: | Simultaneous PRACH/UL_DPCH
| CCH Parameters:
Coder: | Rx Decoder1 #1
Baseband: | Rx Baseband2
RF: | Rx RF #2
| DCH Parameters:
Coder: | Rx Decoder1 #2
Baseband: | Rx Baseband2
RF: | Rx RF #2

#### CPHY BTS Configuration CNF

PHY |  | LLA | @ 00:00:08.670

| BTS unit: |  | 1:1
| CFN: |  | 108

| Message Details:

#### CPHY BTS Configuration CNF

PHY |  | LLA | @ 00:00:08.680

| BTS unit: |  | 1:2
| CFN: |  | 109

| Message Details:

#### CPHY BTS Attenuation REQ

LLA |  | PHY | @ 00:00:08.710

| BTS unit: |  | 1:1
| CFN: |  | 112

| Message Details:
| Configuration Parameters:
Tx Attenuation In dB: | 5
Rx Reference Power In dBm: | 0

#### CPHY BTS Attenuation CNF

PHY |  | LLA | @ 00:00:08.710

| BTS unit: |  | 1:1
| CFN: |  | 112

| Message Details:

#### CPHY BTS Attenuation REQ

LLA |  | PHY | @ 00:00:08.870

| BTS unit: |  | 1:2
| CFN: |  | 128

| Message Details:
| Configuration Parameters:
Tx Attenuation In dB: | 5
Rx Reference Power In dBm: | 0

#### CPHY BTS Attenuation CNF

PHY |  | LLA | @ 00:00:08.870

| BTS unit: |  | 1:2
| CFN: |  | 128

| Message Details:

#### CPHY_Ini_CNF

LLA |  | RRC | @ 00:00:08.880

| Message Details:
| CPHY_Ini_CNF:
confirmation: |

#### CPHY_Cell_Config_REQ

RRC |  | LLA | @ 00:00:08.880

| Cell ID: |  | 0

| Message Details:
| CPHY_Cell_Config_REQ:
cellId: | 0
tcell: | 0
sfnOffset: | 0
| frequencyInfo:
| modeSpecificInfo:
| fdd: (FrequencyInfoFDD)
uarfcn_UL (UARFCN): | Omit
uarfcn_DL (UARFCN): | 10700
primaryScramblingCode_SS: | 100
| cellTxPowerLevel:
defaultCellTxPowerLvl: |
dLTxAttenuationLevel: | 0

#### CPHY BTS Frequency REQ

LLA |  | PHY | @ 00:00:09.030

| BTS unit: |  | 1:1
| CFN: |  | 144

| Message Details:
| Configuration Parameters:
Down Link Frequency: | 2140000000
Up Link Frequency: | 1950000000

#### CPHY BTS Frequency CNF

PHY |  | LLA | @ 00:00:09.030

| BTS unit: |  | 1:1
| CFN: |  | 144

| Message Details:

#### CPHY_Cell_Config_CNF

LLA |  | RRC | @ 00:00:09.050

| Cell ID: |  | 0

| Message Details:
| CPHY_Cell_Config_CNF:
cellId: | 0

#### CPHY_RL_Setup_REQ

RRC |  | LLA | @ 00:00:09.050

| Channel ID: |  | P-CPICH
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_REQ:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 0
ratType: | fdd
| setupMessage: (CphyRlSetupReq)
| physicalChannelInfo:
| primaryCPICHInfo:
dl_TxPower_PCPICH: | -60
txdiversityIndicator: | false

#### CPHY Radio Link Setup REQ

LLA |  | PHY | @ 00:00:09.110

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: P_CPICH
| CFN: |  | 152

| Message Details:
| Configuration Parameters:
Channel Offset: | 7680
Scrambling Code: | 1600
Symbol Rate: | 15k
Channelization Code: | 0
Adjust Time: | 0
Power in dBm: | -40
Tx Diversity: | Off
NumOfDpdch: | 0

#### CPHY Radio Link Setup CNF

PHY |  | LLA | @ 00:00:09.110

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: P_CPICH
| CFN: |  | 152

| Message Details:

#### CPHY_RL_Setup_CNF

LLA |  | RRC | @ 00:00:09.130

| Channel ID: |  | P-CPICH
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_CNF:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 0

#### CPHY_RL_Setup_REQ

RRC |  | LLA | @ 00:00:09.130

| Channel ID: |  | P-SCH
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_REQ:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 1
ratType: | fdd
| setupMessage: (CphyRlSetupReq)
| physicalChannelInfo:
| primarySCHInfo:
tstdIndicator: | false
dl_TxPower: | -5

#### CPHY Radio Link Setup REQ

LLA |  | PHY | @ 00:00:09.190

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: P_SCH
| CFN: |  | 160

| Message Details:
| Configuration Parameters:
Channel Offset: | 7680
Adjust Time: | 0
Power in dBm: | -45
Tx Diversity: | Off
NumOfDpdch: | 0

#### CPHY Radio Link Setup CNF

PHY |  | LLA | @ 00:00:09.190

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: P_SCH
| CFN: |  | 160

| Message Details:

#### CPHY_RL_Setup_CNF

LLA |  | RRC | @ 00:00:09.210

| Channel ID: |  | P-SCH
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_CNF:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 1

#### CPHY_RL_Setup_REQ

RRC |  | LLA | @ 00:00:09.210

| Channel ID: |  | S-SCH
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_REQ:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 2
ratType: | fdd
| setupMessage: (CphyRlSetupReq)
| physicalChannelInfo:
| secondarySCHInfo:
tstdIndicator: | false
dl_TxPower: | -5

#### CPHY Radio Link Setup REQ

LLA |  | PHY | @ 00:00:09.320

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: S_SCH
| CFN: |  | 173

| Message Details:
| Configuration Parameters:
Channel Offset: | 7680
Adjust Time: | 0
Power in dBm: | -45
Tx Diversity: | Off
NumOfDpdch: | 0

#### CPHY Radio Link Setup CNF

PHY |  | LLA | @ 00:00:09.320

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: S_SCH
| CFN: |  | 173

| Message Details:

#### CPHY_RL_Setup_CNF

LLA |  | RRC | @ 00:00:09.350

| Channel ID: |  | S-SCH
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_CNF:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 2

#### CPHY_RL_Setup_REQ

RRC |  | LLA | @ 00:00:09.350

| Channel ID: |  | P-CCPCH
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_REQ:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 4
ratType: | fdd
| setupMessage: (CphyRlSetupReq)
| physicalChannelInfo:
| primaryCCPCHInfo:
sttd_Indicator: | false
dl_TxPower: | -2

#### CPHY Radio Link Setup REQ

LLA |  | PHY | @ 00:00:09.510

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: P_CCPCH
| CFN: |  | 192

| Message Details:
| Configuration Parameters:
Channel Offset: | 7680
SFN Offset: | 0
Scrambling Code: | 1600
Symbol Rate: | 15k
Channelization Code: | 1
Adjust Time: | 0
Power in dBm: | -42
Tx Diversity: | Off
NumOfDpdch: | 1

#### CPHY Radio Link Setup CNF

PHY |  | LLA | @ 00:00:09.510

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: P_CCPCH
| CFN: |  | 192

| Message Details:

#### CPHY_RL_Setup_CNF

LLA |  | RRC | @ 00:00:09.520

| Channel ID: |  | P-CCPCH
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_CNF:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 4

#### CPHY_TrCH_Config_REQ

RRC |  | LLA | @ 00:00:09.520

| Channel ID: |  | P-CCPCH
| Cell ID: |  | 0

| Message Details:
| CPHY_TrCH_Config_REQ:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 4
ratType: | fdd
| trchConfigType:
nonDch: |
| configMessage: (CphyTrchConfigReq)
| activationTime: (SS_ActivationTime)
activateNow: |
| ulconnectedTrCHList: Omit
| ulTFCS: (TFCS) Omit
| dlconnectedTrCHList:
| :
trchid (TransportChannelIdentity): | 11
dl_TransportChannelType (SS_DL_TransportChannelType): | bch
| transportChannelInfo: (CommonOrDedicatedTFS)
| tti:
| tti20: (CommonOrDedicatedTF_InfoList)
| CommonOrDedicatedTF_Info:
tb_Size: | 246
| numberOfTbSizeList:
| NumberOfTransportBlocks:
one: |
| logicalChannelList:
configured: |
| semistaticTF_Information:
| channelCodingType:
convolutional (CodingRate): | half
rateMatchingAttribute: | 1
crc_Size: | crc16
| dlTFCS: (TFCS)
| normalTFCI_Signalling: (ExplicitTFCS_Configuration)
| complete: (TFCS_ReconfAdd)
| ctfcSize:
| ctfc2Bit:
| :
ctfc2: | 0
| powerOffsetInformation:
| gainFactorInformation:
| signalledGainFactors:
| modeSpecificInfo:
| fdd:
gainFactorBetaC (GainFactor): | 11
gainFactorBetaD (GainFactor): | 15
referenceTFC_ID: | 0
powerOffsetPp_m: | Omit

#### CPHY Transport Channel Configuration REQ

LLA |  | PHY | @ 00:00:09.540

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: P_CCPCH
| CFN: |  | 195

| Message Details:
| Configuration Parameters:
DTX Position: | Flexible
Second Interleave: | On
Puncture Limit: | 0
CCTrCH Length: | 270
Number Of Transport Channels: | 1
| Transport Channels:
| Item Number 0:
| Transport Channel Parameters:
| Transport Channel:
Name: | BCH
Identity: | 0
TTI (ms): | 20
EP Type: | 1/2 Rate Convolutional Coding
CRC Size: | 16
RM Attribute: | 1
First Interleave: | On
Number Of Transport Formats: | 2
| Transport Format Set:
| Transport Format 0:
Number Of Transport Blocks: | 0
Transport Block Size In Bits: | 0
| Transport Format 1:
Number Of Transport Blocks: | 1
Transport Block Size In Bits: | 246
RM Maximum Length: | 540
| Transport Format Combination Set:
Number Of Transport Format Combinations: | 2
| Transport Format Combinations 0:
Transport Format: | 0
| Transport Format Combinations 1:
Transport Format: | 1

#### CPHY Transport Channel Configuration CNF

PHY |  | LLA | @ 00:00:09.540

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: P_CCPCH
| CFN: |  | 195

| Message Details:

#### CPHY_TrCH_Config_CNF

LLA |  | RRC | @ 00:00:09.550

| Channel ID: |  | P-CCPCH
| Cell ID: |  | 0

| Message Details:
| CPHY_TrCH_Config_CNF:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 4

#### CMAC_Config_REQ

RRC |  | LLA | @ 00:00:09.550

| Channel ID: |  | P-CCPCH
| Cell ID: |  | 0

| Message Details:
| CMAC_Config_REQ:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 4
ratType: | fdd
| configMessage:
| setup: (CmacConfigReq)
| activationTime: (SS_ActivationTime)
activateNow: |
| uE_Info:
| u_RNTI: Omit
c_RNTI: | Omit
| trCHInfo:
| ulconnectedTrCHList: Omit
| ulTFCS: (TFCS) Omit
| dlconnectedTrCHList:
| :
trchid (TransportChannelIdentity): | 11
| transportChannelInfo: (CommonOrDedicatedTFS)
| tti:
| tti20: (CommonOrDedicatedTF_InfoList)
| CommonOrDedicatedTF_Info:
tb_Size: | 246
| numberOfTbSizeList:
| NumberOfTransportBlocks:
one: |
| logicalChannelList:
configured: |
| semistaticTF_Information:
| channelCodingType:
convolutional (CodingRate): | half
rateMatchingAttribute: | 1
crc_Size: | crc16
| dlTFCS: (TFCS)
| normalTFCI_Signalling: (ExplicitTFCS_Configuration)
| complete: (TFCS_ReconfAdd)
| ctfcSize:
| ctfc2Bit:
| :
ctfc2: | 0
| powerOffsetInformation:
| gainFactorInformation:
| signalledGainFactors:
| modeSpecificInfo:
| fdd:
gainFactorBetaC (GainFactor): | 11
gainFactorBetaD (GainFactor): | 15
referenceTFC_ID: | 0
powerOffsetPp_m: | Omit
| trCH_LogCHMapping: (TrCH_LogCHMappingList1)
| ulconnectedTrCHList: Omit
| dlconnectedTrCHList:
| :
trchid (TransportChannelIdentity): | 11
| trCH_LogCHMappingList:
| TrCH_LogicalChannelMapping:
| logicalChannel_Mapping:
| dl_LogicalChannelMapping: (SS_DL_LogicalChannelMapping)
macHeaderManipulation (MAC_HeaderManipulation): | normalMacHeader
dl_TransportChannelType (SS_DL_TransportChannelType): | bch
logicalChannelIdentity: | 1
logicalChannelType: | bCCH
| rlc_SizeList:
configured: |
mac_LogicalChannelPriority: | 1
rB_Identity: | -1
cn_DomainIdentity: | Omit

#### CMAC Configuration REQ

LLA |  | MAC | @ 00:00:09.570

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: P_CCPCH
| CFN: |  | 198

| Message Details:
| Configuration Parameters:
Number Of Transport Channels: | 1
| Transport Channels:
| Item Number 0:
| Transport Channel Parameters:
| Transport Channel:
Name: | BCH
Identity: | 0
TTI (ms): | 20
EP Type: | 1/2 Rate Convolutional Coding
CRC Size: | 16
RM Attribute: | 1
First Interleave: | On
Number Of Transport Formats: | 2
| Transport Format Set:
| Transport Format 0:
Number Of Transport Blocks: | 0
Transport Block Size In Bits: | 0
| Transport Format 1:
Number Of Transport Blocks: | 1
Transport Block Size In Bits: | 246
Number Of Logical Channels: | 1
| Logical Channels:
| Item Number 0:
| Logical Channel:
Name: | BCCH
Identity: | 0
Priority: | 1
CT Length: | 0
CT Value: | 0
TCTF Length: | 0
TCTF Value: | 0
UE ID Type: | Not used
UE ID: | 0
Active Flag: | 1
| Transport Format Combination Set:
Number Of Transport Format Combinations: | 2
| Transport Format Combinations 0:
Transport Format: | 0
| Transport Format Combinations 1:
Transport Format: | 1

#### CMAC Configuration CNF

MAC |  | LLA | @ 00:00:09.570

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: P_CCPCH
| CFN: |  | 198

| Message Details:

#### CMAC_Config_CNF

LLA |  | RRC | @ 00:00:09.580

| Channel ID: |  | P-CCPCH
| Cell ID: |  | 0

| Message Details:
| CMAC_Config_CNF:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 4

#### CPHY_RL_Setup_REQ

RRC |  | LLA | @ 00:00:09.580

| Channel ID: |  | S-CCPCH#1
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_REQ:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 5
ratType: | fdd
| setupMessage: (CphyRlSetupReq)
| physicalChannelInfo:
| secondaryCCPCHInfo:
scramblingCode: | 0
| dl_ChannelizationCode: (SF256_AndCodeNumber)
sf64: | 1
sCCPCHSlotFormat: | 8
timingOffset: | 0
positionFixedOrFlexible: | flexible
sttd_Indicator: | false
dl_TxPower: | -2
powerOffsetOfTFCI_PO1: | 6
powerOffsetOfPILOT_PO3: | 6

#### CPHY Radio Link Setup REQ

LLA |  | PHY | @ 00:00:09.670

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: S_CCPCH
| CFN: |  | 208

| Message Details:
| Configuration Parameters:
Channel Offset: | 7680
Scrambling Code: | 1600
Symbol Rate: | 60k
Channelization Code: | 1
Adjust Time: | 0
Power in dBm: | -42
Tx Diversity: | Off
Slot Format: | 8
NumOfDpdch: | 1

#### CPHY Radio Link Setup CNF

PHY |  | LLA | @ 00:00:09.670

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: S_CCPCH
| CFN: |  | 208

| Message Details:

#### CPHY_RL_Setup_CNF

LLA |  | RRC | @ 00:00:09.690

| Channel ID: |  | S-CCPCH#1
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_CNF:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 5

#### CPHY_TrCH_Config_REQ

RRC |  | LLA | @ 00:00:09.690

| Channel ID: |  | S-CCPCH#1
| Cell ID: |  | 0

| Message Details:
| CPHY_TrCH_Config_REQ:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 5
ratType: | fdd
| trchConfigType:
nonDch: |
| configMessage: (CphyTrchConfigReq)
| activationTime: (SS_ActivationTime)
activateNow: |
| ulconnectedTrCHList: Omit
| ulTFCS: (TFCS) Omit
| dlconnectedTrCHList:
| :
trchid (TransportChannelIdentity): | 12
dl_TransportChannelType (SS_DL_TransportChannelType): | pch
| transportChannelInfo: (CommonOrDedicatedTFS)
| tti:
| tti10: (CommonOrDedicatedTF_InfoList)
| CommonOrDedicatedTF_Info:
tb_Size: | 240
| numberOfTbSizeList:
| NumberOfTransportBlocks:
zero: |
| NumberOfTransportBlocks:
one: |
| logicalChannelList:
allSizes: |
| semistaticTF_Information:
| channelCodingType:
convolutional (CodingRate): | half
rateMatchingAttribute: | 230
crc_Size: | crc16
| :
trchid (TransportChannelIdentity): | 13
dl_TransportChannelType (SS_DL_TransportChannelType): | fach
| transportChannelInfo: (CommonOrDedicatedTFS)
| tti:
| tti10: (CommonOrDedicatedTF_InfoList)
| CommonOrDedicatedTF_Info:
tb_Size: | 168
| numberOfTbSizeList:
| NumberOfTransportBlocks:
zero: |
| NumberOfTransportBlocks:
one: |
| NumberOfTransportBlocks:
small: | 2
| logicalChannelList:
allSizes: |
| semistaticTF_Information:
| channelCodingType:
convolutional (CodingRate): | half
rateMatchingAttribute: | 220
crc_Size: | crc16
| :
trchid (TransportChannelIdentity): | 14
dl_TransportChannelType (SS_DL_TransportChannelType): | fach
| transportChannelInfo: (CommonOrDedicatedTFS)
| tti:
| tti10: (CommonOrDedicatedTF_InfoList)
| CommonOrDedicatedTF_Info:
tb_Size: | 360
| numberOfTbSizeList:
| NumberOfTransportBlocks:
zero: |
| NumberOfTransportBlocks:
one: |
| logicalChannelList:
allSizes: |
| semistaticTF_Information:
| channelCodingType:
turbo: |
rateMatchingAttribute: | 130
crc_Size: | crc16
| dlTFCS: (TFCS)
| normalTFCI_Signalling: (ExplicitTFCS_Configuration)
| complete: (TFCS_ReconfAdd)
| ctfcSize:
| ctfc4Bit:
| :
ctfc4: | 0
| powerOffsetInformation:
| gainFactorInformation:
computedGainFactors (ReferenceTFC_ID): | 0
powerOffsetPp_m: | Omit
| :
ctfc4: | 1
| powerOffsetInformation:
| gainFactorInformation:
computedGainFactors (ReferenceTFC_ID): | 0
powerOffsetPp_m: | Omit
| :
ctfc4: | 2
| powerOffsetInformation:
| gainFactorInformation:
computedGainFactors (ReferenceTFC_ID): | 0
powerOffsetPp_m: | Omit
| :
ctfc4: | 3
| powerOffsetInformation:
| gainFactorInformation:
computedGainFactors (ReferenceTFC_ID): | 0
powerOffsetPp_m: | Omit
| :
ctfc4: | 4
| powerOffsetInformation:
| gainFactorInformation:
computedGainFactors (ReferenceTFC_ID): | 0
powerOffsetPp_m: | Omit
| :
ctfc4: | 5
| powerOffsetInformation:
| gainFactorInformation:
computedGainFactors (ReferenceTFC_ID): | 0
powerOffsetPp_m: | Omit
| :
ctfc4: | 6
| powerOffsetInformation:
| gainFactorInformation:
computedGainFactors (ReferenceTFC_ID): | 0
powerOffsetPp_m: | Omit
| :
ctfc4: | 8
| powerOffsetInformation:
| gainFactorInformation:
| signalledGainFactors:
| modeSpecificInfo:
| fdd:
gainFactorBetaC (GainFactor): | 11
gainFactorBetaD (GainFactor): | 15
referenceTFC_ID: | 0
powerOffsetPp_m: | Omit

#### CPHY Transport Channel Configuration REQ

LLA |  | PHY | @ 00:00:09.710

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: S_CCPCH
| CFN: |  | 212

| Message Details:
| Configuration Parameters:
DTX Position: | Flexible
Second Interleave: | On
Puncture Limit: | 100
CCTrCH Length: | 1080
Number Of Transport Channels: | 3
| Transport Channels:
| Item Number 0:
| Transport Channel Parameters:
| Transport Channel:
Name: | PCH
Identity: | 0
TTI (ms): | 10
EP Type: | 1/2 Rate Convolutional Coding
CRC Size: | 16
RM Attribute: | 230
First Interleave: | On
Number Of Transport Formats: | 2
| Transport Format Set:
| Transport Format 0:
Number Of Transport Blocks: | 0
Transport Block Size In Bits: | 240
| Transport Format 1:
Number Of Transport Blocks: | 1
Transport Block Size In Bits: | 240
RM Maximum Length: | 457
| Item Number 1:
| Transport Channel Parameters:
| Transport Channel:
Name: | FACH
Identity: | 0
TTI (ms): | 10
EP Type: | 1/2 Rate Convolutional Coding
CRC Size: | 16
RM Attribute: | 220
First Interleave: | On
Number Of Transport Formats: | 3
| Transport Format Set:
| Transport Format 0:
Number Of Transport Blocks: | 0
Transport Block Size In Bits: | 168
| Transport Format 1:
Number Of Transport Blocks: | 1
Transport Block Size In Bits: | 168
| Transport Format 2:
Number Of Transport Blocks: | 2
Transport Block Size In Bits: | 168
RM Maximum Length: | 623
| Item Number 2:
| Transport Channel Parameters:
| Transport Channel:
Name: | FACH
Identity: | 1
TTI (ms): | 10
EP Type: | Turbo Coding
CRC Size: | 16
RM Attribute: | 130
First Interleave: | On
Number Of Transport Formats: | 2
| Transport Format Set:
| Transport Format 0:
Number Of Transport Blocks: | 0
Transport Block Size In Bits: | 360
| Transport Format 1:
Number Of Transport Blocks: | 1
Transport Block Size In Bits: | 360
RM Maximum Length: | 558
| Transport Format Combination Set:
Number Of Transport Format Combinations: | 8
| Transport Format Combinations 0:
Transport Format: | 0
Transport Format: | 0
Transport Format: | 0
| Transport Format Combinations 1:
Transport Format: | 1
Transport Format: | 0
Transport Format: | 0
| Transport Format Combinations 2:
Transport Format: | 0
Transport Format: | 1
Transport Format: | 0
| Transport Format Combinations 3:
Transport Format: | 1
Transport Format: | 1
Transport Format: | 0
| Transport Format Combinations 4:
Transport Format: | 0
Transport Format: | 2
Transport Format: | 0
| Transport Format Combinations 5:
Transport Format: | 1
Transport Format: | 2
Transport Format: | 0
| Transport Format Combinations 6:
Transport Format: | 0
Transport Format: | 0
Transport Format: | 1
| Transport Format Combinations 7:
Transport Format: | 0
Transport Format: | 1
Transport Format: | 1

#### CPHY Transport Channel Configuration CNF

PHY |  | LLA | @ 00:00:09.710

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: S_CCPCH
| CFN: |  | 212

| Message Details:

#### CPHY_TrCH_Config_CNF

LLA |  | RRC | @ 00:00:09.720

| Channel ID: |  | S-CCPCH#1
| Cell ID: |  | 0

| Message Details:
| CPHY_TrCH_Config_CNF:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 5

#### CMAC_Config_REQ

RRC |  | LLA | @ 00:00:09.720

| Channel ID: |  | S-CCPCH#1
| Cell ID: |  | 0

| Message Details:
| CMAC_Config_REQ:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 5
ratType: | fdd
| configMessage:
| setup: (CmacConfigReq)
| activationTime: (SS_ActivationTime)
activateNow: |
| uE_Info:
| u_RNTI: Omit
c_RNTI: | Omit
| trCHInfo:
| ulconnectedTrCHList: Omit
| ulTFCS: (TFCS) Omit
| dlconnectedTrCHList:
| :
trchid (TransportChannelIdentity): | 12
| transportChannelInfo: (CommonOrDedicatedTFS)
| tti:
| tti10: (CommonOrDedicatedTF_InfoList)
| CommonOrDedicatedTF_Info:
tb_Size: | 240
| numberOfTbSizeList:
| NumberOfTransportBlocks:
zero: |
| NumberOfTransportBlocks:
one: |
| logicalChannelList:
allSizes: |
| semistaticTF_Information:
| channelCodingType:
convolutional (CodingRate): | half
rateMatchingAttribute: | 230
crc_Size: | crc16
| :
trchid (TransportChannelIdentity): | 13
| transportChannelInfo: (CommonOrDedicatedTFS)
| tti:
| tti10: (CommonOrDedicatedTF_InfoList)
| CommonOrDedicatedTF_Info:
tb_Size: | 168
| numberOfTbSizeList:
| NumberOfTransportBlocks:
zero: |
| NumberOfTransportBlocks:
one: |
| NumberOfTransportBlocks:
small: | 2
| logicalChannelList:
allSizes: |
| semistaticTF_Information:
| channelCodingType:
convolutional (CodingRate): | half
rateMatchingAttribute: | 220
crc_Size: | crc16
| :
trchid (TransportChannelIdentity): | 14
| transportChannelInfo: (CommonOrDedicatedTFS)
| tti:
| tti10: (CommonOrDedicatedTF_InfoList)
| CommonOrDedicatedTF_Info:
tb_Size: | 360
| numberOfTbSizeList:
| NumberOfTransportBlocks:
zero: |
| NumberOfTransportBlocks:
one: |
| logicalChannelList:
allSizes: |
| semistaticTF_Information:
| channelCodingType:
turbo: |
rateMatchingAttribute: | 130
crc_Size: | crc16
| dlTFCS: (TFCS)
| normalTFCI_Signalling: (ExplicitTFCS_Configuration)
| complete: (TFCS_ReconfAdd)
| ctfcSize:
| ctfc4Bit:
| :
ctfc4: | 0
| powerOffsetInformation:
| gainFactorInformation:
computedGainFactors (ReferenceTFC_ID): | 0
powerOffsetPp_m: | Omit
| :
ctfc4: | 1
| powerOffsetInformation:
| gainFactorInformation:
computedGainFactors (ReferenceTFC_ID): | 0
powerOffsetPp_m: | Omit
| :
ctfc4: | 2
| powerOffsetInformation:
| gainFactorInformation:
computedGainFactors (ReferenceTFC_ID): | 0
powerOffsetPp_m: | Omit
| :
ctfc4: | 3
| powerOffsetInformation:
| gainFactorInformation:
computedGainFactors (ReferenceTFC_ID): | 0
powerOffsetPp_m: | Omit
| :
ctfc4: | 4
| powerOffsetInformation:
| gainFactorInformation:
computedGainFactors (ReferenceTFC_ID): | 0
powerOffsetPp_m: | Omit
| :
ctfc4: | 5
| powerOffsetInformation:
| gainFactorInformation:
computedGainFactors (ReferenceTFC_ID): | 0
powerOffsetPp_m: | Omit
| :
ctfc4: | 6
| powerOffsetInformation:
| gainFactorInformation:
computedGainFactors (ReferenceTFC_ID): | 0
powerOffsetPp_m: | Omit
| :
ctfc4: | 8
| powerOffsetInformation:
| gainFactorInformation:
| signalledGainFactors:
| modeSpecificInfo:
| fdd:
gainFactorBetaC (GainFactor): | 11
gainFactorBetaD (GainFactor): | 15
referenceTFC_ID: | 0
powerOffsetPp_m: | Omit
| trCH_LogCHMapping: (TrCH_LogCHMappingList1)
| ulconnectedTrCHList: Omit
| dlconnectedTrCHList:
| :
trchid (TransportChannelIdentity): | 12
| trCH_LogCHMappingList:
| TrCH_LogicalChannelMapping:
| logicalChannel_Mapping:
| dl_LogicalChannelMapping: (SS_DL_LogicalChannelMapping)
macHeaderManipulation (MAC_HeaderManipulation): | normalMacHeader
dl_TransportChannelType (SS_DL_TransportChannelType): | pch
logicalChannelIdentity: | 1
logicalChannelType: | pCCH
| rlc_SizeList:
configured: |
mac_LogicalChannelPriority: | 1
rB_Identity: | -2
cn_DomainIdentity: | Omit
| :
trchid (TransportChannelIdentity): | 13
| trCH_LogCHMappingList:
| TrCH_LogicalChannelMapping:
| logicalChannel_Mapping:
| dl_LogicalChannelMapping: (SS_DL_LogicalChannelMapping)
macHeaderManipulation (MAC_HeaderManipulation): | normalMacHeader
dl_TransportChannelType (SS_DL_TransportChannelType): | fach
logicalChannelIdentity: | 5
logicalChannelType: | cCCH
| rlc_SizeList:
configured: |
mac_LogicalChannelPriority: | 1
rB_Identity: | 0
cn_DomainIdentity: | Omit

#### CMAC_Config_CNF

LLA |  | RRC | @ 00:00:09.740

| Channel ID: |  | S-CCPCH#1
| Cell ID: |  | 0

| Message Details:
| CMAC_Config_CNF:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 5

#### CPHY_RL_Setup_REQ

RRC |  | LLA | @ 00:00:09.740

| Channel ID: |  | PICH#1
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_REQ:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 6
ratType: | fdd
| setupMessage: (CphyRlSetupReq)
| physicalChannelInfo:
| pICHInfo:
| pichinfo: (PICH_Info)
| fdd:
channelisationCode256: | 2
pi_CountPerFrame: | e18
sttd_Indicator: | false
dl_TxPower (PICH_PowerOffset): | -5
sccpchId_associated: | 5

#### CPHY Radio Link Setup REQ

LLA |  | PHY | @ 00:00:09.760

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: PICH
| CFN: |  | 217

| Message Details:
| Configuration Parameters:
Channel Offset: | 0
Scrambling Code: | 1600
Symbol Rate: | 15k
Channelization Code: | 2
Adjust Time: | 0
Power in dBm: | -45
Tx Diversity: | Off
NumOfDpdch: | 0
Np: | 18

#### CPHY Radio Link Setup CNF

PHY |  | LLA | @ 00:00:09.760

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: PICH
| CFN: |  | 217

| Message Details:

#### CPHY_RL_Setup_CNF

LLA |  | RRC | @ 00:00:09.770

| Channel ID: |  | PICH#1
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_CNF:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 6

#### CPHY_RL_Setup_REQ

RRC |  | LLA | @ 00:00:09.770

| Channel ID: |  | AICH#1
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_REQ:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 7
ratType: | fdd
| setupMessage: (CphyRlSetupReq)
| physicalChannelInfo:
| aICHInfo:
| aichinfo: (AICH_Info)
channelisationCode256: | 3
sttd_Indicator: | false
aich_TransmissionTiming: | e0
dl_TxPower (AICH_PowerOffset): | -5

#### CPHY Radio Link Setup REQ

LLA |  | PHY | @ 00:00:09.830

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: AICH
| CFN: |  | 224

| Message Details:
| Configuration Parameters:
Channel Offset: | 7680
Scrambling Code: | 1600
Symbol Rate: | 15k
Channelization Code: | 3
Adjust Time: | 0
Power in dBm: | -45
Tx Diversity: | Off
AICH Transmission Timing: | 3 Access Slots
AICH Polarity: | Positive
NumOfDpdch: | 0

#### CPHY Radio Link Setup CNF

PHY |  | LLA | @ 00:00:09.830

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: AICH
| CFN: |  | 224

| Message Details:

#### CPHY_RL_Setup_CNF

LLA |  | RRC | @ 00:00:09.850

| Channel ID: |  | AICH#1
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_CNF:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 7

#### CPHY_RL_Setup_REQ

RRC |  | LLA | @ 00:00:09.850

| Channel ID: |  | PRACH#1
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_REQ:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 8
ratType: | fdd
| setupMessage: (CphyRlSetupReq)
| physicalChannelInfo:
| pRACHInfo:
| fdd_tdd:
| fdd:
preambleSignature (AvailableSignatures): | 0000000011111111
spreadingFactorForDataPart (SF_PRACH): | sfpr64
preambleScramblingCode (PreambleScramblingCodeWordNumber): | 0
puncturingLimit: | pl1
accessSlot (AvailableSubChannelNumbers): | 111111111111

#### CPHY_RL_Setup_CNF

LLA |  | RRC | @ 00:00:09.860

| Channel ID: |  | PRACH#1
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_CNF:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 8

#### CPHY_TrCH_Config_REQ

RRC |  | LLA | @ 00:00:09.860

| Channel ID: |  | PRACH#1
| Cell ID: |  | 0

| Message Details:
| CPHY_TrCH_Config_REQ:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 8
ratType: | fdd
| trchConfigType:
nonDch: |
| configMessage: (CphyTrchConfigReq)
| activationTime: (SS_ActivationTime)
activateNow: |
| ulconnectedTrCHList:
| :
trchid (TransportChannelIdentity): | 15
ul_TransportChannelType (SS_UL_TransportChannelType): | rach
| transportChannelInfo: (CommonOrDedicatedTFS)
| tti:
| tti20: (CommonOrDedicatedTF_InfoList)
| CommonOrDedicatedTF_Info:
tb_Size: | 168
| numberOfTbSizeList:
| NumberOfTransportBlocks:
one: |
| logicalChannelList:
configured: |
| CommonOrDedicatedTF_Info:
tb_Size: | 360
| numberOfTbSizeList:
| NumberOfTransportBlocks:
one: |
| logicalChannelList:
configured: |
| semistaticTF_Information:
| channelCodingType:
convolutional (CodingRate): | half
rateMatchingAttribute: | 150
crc_Size: | crc16
| ulTFCS: (TFCS)
| normalTFCI_Signalling: (ExplicitTFCS_Configuration)
| complete: (TFCS_ReconfAdd)
| ctfcSize:
| ctfc2Bit:
| :
ctfc2: | 0
| powerOffsetInformation: Omit
| :
ctfc2: | 1
| powerOffsetInformation: Omit
| dlconnectedTrCHList: Omit
| dlTFCS: (TFCS) Omit

#### CPHY Radio Link Setup REQ

LLA |  | PHY | @ 00:00:09.970

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: PRACH
| CFN: |  | 238

| Message Details:
| Configuration Parameters:
Channel Offset: | 10240
Scrambling Code: | 16778816
Symbol Rate: | 60k
Channelization Code: | 128
Adjust Time: | 0
Slot Format: | 2
NumOfDpdch: | 1

#### CPHY Radio Link Setup CNF

PHY |  | LLA | @ 00:00:09.970

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: PRACH
| CFN: |  | 238

| Message Details:

#### CPHY Transport Channel Configuration REQ

LLA |  | PHY | @ 00:00:10.020

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: PRACH
| CFN: |  | 243

| Message Details:
| Configuration Parameters:
DTX Position: | Flexible
Second Interleave: | On
Puncture Limit: | 100
CCTrCH Length: | 600
Number Of Transport Channels: | 1
| Transport Channels:
| Item Number 0:
| Transport Channel Parameters:
| Transport Channel:
Name: | RACH
Identity: | 0
TTI (ms): | 20
EP Type: | 1/2 Rate Convolutional Coding
CRC Size: | 16
RM Attribute: | 150
First Interleave: | On
Number Of Transport Formats: | 2
| Transport Format Set:
| Transport Format 0:
Number Of Transport Blocks: | 1
Transport Block Size In Bits: | 168
| Transport Format 1:
Number Of Transport Blocks: | 1
Transport Block Size In Bits: | 360
RM Maximum Length: | 600
| Transport Format Combination Set:
Number Of Transport Format Combinations: | 2
| Transport Format Combinations 0:
Transport Format: | 0
| Transport Format Combinations 1:
Transport Format: | 1

#### CPHY Transport Channel Configuration CNF

PHY |  | LLA | @ 00:00:10.040

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: PRACH
| CFN: |  | 245

| Message Details:

#### CPHY_TrCH_Config_CNF

LLA |  | RRC | @ 00:00:10.070

| Channel ID: |  | PRACH#1
| Cell ID: |  | 0

| Message Details:
| CPHY_TrCH_Config_CNF:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 8

#### CMAC_Config_REQ

RRC |  | LLA | @ 00:00:10.070

| Channel ID: |  | PRACH#1
| Cell ID: |  | 0

| Message Details:
| CMAC_Config_REQ:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 8
ratType: | fdd
| configMessage:
| setup: (CmacConfigReq)
| activationTime: (SS_ActivationTime)
activateNow: |
| uE_Info:
| u_RNTI: Omit
c_RNTI: | Omit
| trCHInfo:
| ulconnectedTrCHList:
| :
trchid (TransportChannelIdentity): | 15
| transportChannelInfo: (CommonOrDedicatedTFS)
| tti:
| tti20: (CommonOrDedicatedTF_InfoList)
| CommonOrDedicatedTF_Info:
tb_Size: | 168
| numberOfTbSizeList:
| NumberOfTransportBlocks:
one: |
| logicalChannelList:
configured: |
| CommonOrDedicatedTF_Info:
tb_Size: | 360
| numberOfTbSizeList:
| NumberOfTransportBlocks:
one: |
| logicalChannelList:
configured: |
| semistaticTF_Information:
| channelCodingType:
convolutional (CodingRate): | half
rateMatchingAttribute: | 150
crc_Size: | crc16
| ulTFCS: (TFCS)
| normalTFCI_Signalling: (ExplicitTFCS_Configuration)
| complete: (TFCS_ReconfAdd)
| ctfcSize:
| ctfc2Bit:
| :
ctfc2: | 0
| powerOffsetInformation: Omit
| :
ctfc2: | 1
| powerOffsetInformation: Omit
| dlconnectedTrCHList: Omit
| dlTFCS: (TFCS) Omit
| trCH_LogCHMapping: (TrCH_LogCHMappingList1)
| ulconnectedTrCHList:
| :
trchid (TransportChannelIdentity): | 15
| trCH_LogCHMappingList:
| TrCH_LogicalChannelMapping:
| logicalChannel_Mapping:
| ul_LogicalChannelMapping: (SS_UL_LogicalChannelMapping)
macHeaderManipulation (MAC_HeaderManipulation): | normalMacHeader
ul_TransportChannelType (SS_UL_TransportChannelType): | rach
logicalChannelIdentity: | 5
logicalChannelType: | cCCH
rB_Identity: | 0
cn_DomainIdentity: | Omit
| dlconnectedTrCHList: Omit

#### CMAC Configuration REQ

LLA |  | MAC | @ 00:00:10.090

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: PRACH
| CFN: |  | 250

| Message Details:
| Configuration Parameters:
Number Of Transport Channels: | 1
| Transport Channels:
| Item Number 0:
| Transport Channel Parameters:
| Transport Channel:
Name: | RACH
Identity: | 0
TTI (ms): | 20
EP Type: | 1/2 Rate Convolutional Coding
CRC Size: | 16
RM Attribute: | 150
First Interleave: | On
Number Of Transport Formats: | 2
| Transport Format Set:
| Transport Format 0:
Number Of Transport Blocks: | 1
Transport Block Size In Bits: | 168
| Transport Format 1:
Number Of Transport Blocks: | 1
Transport Block Size In Bits: | 360
Number Of Logical Channels: | 1
| Logical Channels:
| Item Number 0:
| Logical Channel:
Name: | CCCH
Identity: | 0
Priority: | 0
CT Length: | 0
CT Value: | 0
TCTF Length: | 2
TCTF Value: | 0
UE ID Type: | Not used
UE ID: | 0
Active Flag: | 1
| Transport Format Combination Set:
Number Of Transport Format Combinations: | 2
| Transport Format Combinations 0:
Transport Format: | 0
| Transport Format Combinations 1:
Transport Format: | 1

#### CMAC Configuration CNF

MAC |  | LLA | @ 00:00:10.090

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: PRACH
| CFN: |  | 250

| Message Details:

#### CMAC_Config_CNF

LLA |  | RRC | @ 00:00:10.110

| Channel ID: |  | PRACH#1
| Cell ID: |  | 0

| Message Details:
| CMAC_Config_CNF:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 8

#### CPHY_RL_Setup_REQ

RRC |  | LLA | @ 00:00:10.110

| Channel ID: |  | DL-DPCH#1
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_REQ:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 26
ratType: | fdd
| setupMessage: (CphyRlSetupReq)
| physicalChannelInfo:
| dPCHInfo:
| ul_DPCHInfo: (UL_DPCH_Info) Omit
| dl_DPCHInfo:
| dl_CommonInformation:
| dl_DPCH_InfoCommon:
| cfnHandling:
| initialise:
cfntargetsfnframeoffset: | Omit
| modeSpecificInfo:
| fdd:
| dl_DPCH_PowerControlInfo:
| modeSpecificInfo:
| fdd:
dpc_Mode: | singleTPC
powerOffsetPilot_pdpdch: | 0
| dl_rate_matching_restriction: Omit
| spreadingFactorAndPilot: (SF512_AndPilot)
sfd128 (PilotBits128): | pb4
positionFixedOrFlexible: | fixed
tfci_Existence: | false
| modeSpecificInfo:
| fdd:
defaultDPCH_OffsetValue (DefaultDPCH_OffsetValueFDD): | 0
| dpch_CompressedModeInfo: Omit
tx_DiversityMode: | noDiversity
| ssdt_Information: Omit
| dl_DPCH_InfoPerRL:
| fdd:
pCPICH_UsageForChannelEst: | mayBeUsed
dpch_FrameOffset: | 0
| secondaryCPICH_Info: Omit
| dl_ChannelisationCodeList:
| DL_ChannelisationCode:
secondaryScramblingCode: | 1
| sf_AndCodeNumber: (SF512_AndCodeNumber)
sf128: | 0
scramblingCodeChange: | Omit
tpc_CombinationIndex: | 0
ssdt_CellIdentity: | Omit
closedLoopTimingAdjMode: | Omit
powerOffsetOfTFCI_PO1: | 0
powerOffsetOfTPC_PO2: | 0
powerOffsetOfPILOT_PO3: | 0
dl_TxPower: | -5
dl_TxPowerMax (DL_TxPower): | 15
dl_TxPowerMin (DL_TxPower): | -35

#### CPHY Radio Link Setup REQ

LLA |  | PHY | @ 00:00:10.150

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: D_DPCH
| CFN: |  | 0

| Message Details:
| Configuration Parameters:
Channel Offset: | 7680
Scrambling Code: | 1601
Symbol Rate: | 30k
Channelization Code: | 0
Adjust Time: | 0
Power in dBm: | -45
Tx Diversity: | Off
Slot Format: | 8
Number Of DPDCH: | 1
| DPDCH Parameters:
| Item Number 0:
Power in dBm: | -45
Channelization Code: | 0

#### CPHY Radio Link Setup CNF

PHY |  | LLA | @ 00:00:10.150

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: D_DPCH
| CFN: |  | 0

| Message Details:

#### CPHY_RL_Setup_CNF

LLA |  | RRC | @ 00:00:10.160

| Channel ID: |  | DL-DPCH#1
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_CNF:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 26

#### CPHY_TrCH_Config_REQ

RRC |  | LLA | @ 00:00:10.160

| Channel ID: |  | DL-DPCH#1
| Cell ID: |  | 0

| Message Details:
| CPHY_TrCH_Config_REQ:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 26
ratType: | fdd
| trchConfigType:
dch: | Normal
| configMessage: (CphyTrchConfigReq)
| activationTime: (SS_ActivationTime)
activateNow: |
| ulconnectedTrCHList: Omit
| ulTFCS: (TFCS) Omit
| dlconnectedTrCHList:
| :
trchid (TransportChannelIdentity): | 10
dl_TransportChannelType (SS_DL_TransportChannelType): | dch
| transportChannelInfo: (CommonOrDedicatedTFS)
| tti:
| tti10: (CommonOrDedicatedTF_InfoList)
| CommonOrDedicatedTF_Info:
tb_Size: | 148
| numberOfTbSizeList:
| NumberOfTransportBlocks:
zero: |
| NumberOfTransportBlocks:
one: |
| logicalChannelList:
allSizes: |
| semistaticTF_Information:
| channelCodingType:
convolutional (CodingRate): | third
rateMatchingAttribute: | 192
crc_Size: | crc16
| dlTFCS: (TFCS)
| normalTFCI_Signalling: (ExplicitTFCS_Configuration)
| complete: (TFCS_ReconfAdd)
| ctfcSize:
| ctfc2Bit:
| :
ctfc2: | 0
| powerOffsetInformation:
| gainFactorInformation:
computedGainFactors (ReferenceTFC_ID): | 0
powerOffsetPp_m: | Omit
| :
ctfc2: | 1
| powerOffsetInformation:
| gainFactorInformation:
| signalledGainFactors:
| modeSpecificInfo:
| fdd:
gainFactorBetaC (GainFactor): | 11
gainFactorBetaD (GainFactor): | 15
referenceTFC_ID: | 0
powerOffsetPp_m: | Omit

#### CPHY Transport Channel Configuration REQ

LLA |  | PHY | @ 00:00:10.180

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: D_DPCH
| CFN: |  | 3

| Message Details:
| Configuration Parameters:
DTX Position: | Fixed
Second Interleave: | On
Puncture Limit: | 0
CCTrCH Length: | 510
Number Of Transport Channels: | 1
| Transport Channels:
| Item Number 0:
| Transport Channel Parameters:
| Transport Channel:
Name: | D_DCH
Identity: | 0
TTI (ms): | 10
EP Type: | 1/3 Rate Convolutional Coding
CRC Size: | 16
RM Attribute: | 192
First Interleave: | On
Number Of Transport Formats: | 2
| Transport Format Set:
| Transport Format 0:
Number Of Transport Blocks: | 0
Transport Block Size In Bits: | 148
| Transport Format 1:
Number Of Transport Blocks: | 1
Transport Block Size In Bits: | 148
RM Maximum Length: | 510
| Transport Format Combination Set:
Number Of Transport Format Combinations: | 2
| Transport Format Combinations 0:
Transport Format: | 0
| Transport Format Combinations 1:
Transport Format: | 1

#### CPHY Transport Channel Configuration CNF

PHY |  | LLA | @ 00:00:10.180

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: D_DPCH
| CFN: |  | 3

| Message Details:

#### CPHY_TrCH_Config_CNF

LLA |  | RRC | @ 00:00:10.190

| Channel ID: |  | DL-DPCH#1
| Cell ID: |  | 0

| Message Details:
| CPHY_TrCH_Config_CNF:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 26

#### CMAC_Config_REQ

RRC |  | LLA | @ 00:00:10.190

| Channel ID: |  | DL-DPCH#1
| Cell ID: |  | -1

| Message Details:
| CMAC_Config_REQ:
cellId: | -1
| routingInfo:
physicalChannelIdentity: | 26
ratType: | fdd
| configMessage:
| setup: (CmacConfigReq)
| activationTime: (SS_ActivationTime)
activateNow: |
| uE_Info:
| u_RNTI: Omit
c_RNTI: | Omit
| trCHInfo:
| ulconnectedTrCHList: Omit
| ulTFCS: (TFCS) Omit
| dlconnectedTrCHList:
| :
trchid (TransportChannelIdentity): | 10
| transportChannelInfo: (CommonOrDedicatedTFS)
| tti:
| tti10: (CommonOrDedicatedTF_InfoList)
| CommonOrDedicatedTF_Info:
tb_Size: | 148
| numberOfTbSizeList:
| NumberOfTransportBlocks:
zero: |
| NumberOfTransportBlocks:
one: |
| logicalChannelList:
allSizes: |
| semistaticTF_Information:
| channelCodingType:
convolutional (CodingRate): | third
rateMatchingAttribute: | 192
crc_Size: | crc16
| dlTFCS: (TFCS)
| normalTFCI_Signalling: (ExplicitTFCS_Configuration)
| complete: (TFCS_ReconfAdd)
| ctfcSize:
| ctfc2Bit:
| :
ctfc2: | 0
| powerOffsetInformation:
| gainFactorInformation:
computedGainFactors (ReferenceTFC_ID): | 0
powerOffsetPp_m: | Omit
| :
ctfc2: | 1
| powerOffsetInformation:
| gainFactorInformation:
| signalledGainFactors:
| modeSpecificInfo:
| fdd:
gainFactorBetaC (GainFactor): | 11
gainFactorBetaD (GainFactor): | 15
referenceTFC_ID: | 0
powerOffsetPp_m: | Omit
| trCH_LogCHMapping: (TrCH_LogCHMappingList1)
| ulconnectedTrCHList: Omit
| dlconnectedTrCHList:
| :
trchid (TransportChannelIdentity): | 10
| trCH_LogCHMappingList:
| TrCH_LogicalChannelMapping:
| logicalChannel_Mapping:
| dl_LogicalChannelMapping: (SS_DL_LogicalChannelMapping)
macHeaderManipulation (MAC_HeaderManipulation): | normalMacHeader
dl_TransportChannelType (SS_DL_TransportChannelType): | dch
logicalChannelIdentity: | 1
logicalChannelType: | dCCH
| rlc_SizeList:
configured: |
mac_LogicalChannelPriority: | 1
rB_Identity: | 1
cn_DomainIdentity: | Omit
| TrCH_LogicalChannelMapping:
| logicalChannel_Mapping:
| dl_LogicalChannelMapping: (SS_DL_LogicalChannelMapping)
macHeaderManipulation (MAC_HeaderManipulation): | normalMacHeader
dl_TransportChannelType (SS_DL_TransportChannelType): | dch
logicalChannelIdentity: | 2
logicalChannelType: | dCCH
| rlc_SizeList:
configured: |
mac_LogicalChannelPriority: | 2
rB_Identity: | 2
cn_DomainIdentity: | Omit
| TrCH_LogicalChannelMapping:
| logicalChannel_Mapping:
| dl_LogicalChannelMapping: (SS_DL_LogicalChannelMapping)
macHeaderManipulation (MAC_HeaderManipulation): | normalMacHeader
dl_TransportChannelType (SS_DL_TransportChannelType): | dch
logicalChannelIdentity: | 3
logicalChannelType: | dCCH
| rlc_SizeList:
configured: |
mac_LogicalChannelPriority: | 3
rB_Identity: | 3
cn_DomainIdentity: | Omit
| TrCH_LogicalChannelMapping:
| logicalChannel_Mapping:
| dl_LogicalChannelMapping: (SS_DL_LogicalChannelMapping)
macHeaderManipulation (MAC_HeaderManipulation): | normalMacHeader
dl_TransportChannelType (SS_DL_TransportChannelType): | dch
logicalChannelIdentity: | 4
logicalChannelType: | dCCH
| rlc_SizeList:
configured: |
mac_LogicalChannelPriority: | 4
rB_Identity: | 4
cn_DomainIdentity: | Omit

#### CMAC Configuration REQ

LLA |  | MAC | @ 00:00:10.210

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: D_DPCH
| CFN: |  | 6

| Message Details:
| Configuration Parameters:
Number Of Transport Channels: | 1
| Transport Channels:
| Item Number 0:
| Transport Channel Parameters:
| Transport Channel:
Name: | D_DCH
Identity: | 0
TTI (ms): | 10
EP Type: | 1/3 Rate Convolutional Coding
CRC Size: | 16
RM Attribute: | 192
First Interleave: | On
Number Of Transport Formats: | 2
| Transport Format Set:
| Transport Format 0:
Number Of Transport Blocks: | 0
Transport Block Size In Bits: | 148
| Transport Format 1:
Number Of Transport Blocks: | 1
Transport Block Size In Bits: | 148
Number Of Logical Channels: | 4
| Logical Channels:
| Item Number 0:
| Logical Channel:
Name: | DCCH
Identity: | 1
Priority: | 1
CT Length: | 4
CT Value: | 0
TCTF Length: | 0
TCTF Value: | 0
UE ID Type: | Not used
UE ID: | 0
| Item Number 1:
| Logical Channel:
Name: | DCCH
Identity: | 2
Priority: | 2
CT Length: | 4
CT Value: | 1
TCTF Length: | 0
TCTF Value: | 0
UE ID Type: | Not used
UE ID: | 0
| Item Number 2:
| Logical Channel:
Name: | DCCH
Identity: | 3
Priority: | 3
CT Length: | 4
CT Value: | 2
TCTF Length: | 0
TCTF Value: | 0
UE ID Type: | Not used
UE ID: | 0
| Item Number 3:
| Logical Channel:
Name: | DCCH
Identity: | 4
Priority: | 4
CT Length: | 4
CT Value: | 3
TCTF Length: | 0
TCTF Value: | 0
UE ID Type: | Not used
UE ID: | 0
Active Flag: | 1
| Transport Format Combination Set:
Number Of Transport Format Combinations: | 2
| Transport Format Combinations 0:
Transport Format: | 0
| Transport Format Combinations 1:
Transport Format: | 1

#### CMAC Configuration CNF

MAC |  | LLA | @ 00:00:10.210

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: D_DPCH
| CFN: |  | 6

| Message Details:

#### CMAC_Config_CNF

LLA |  | RRC | @ 00:00:10.240

| Channel ID: |  | DL-DPCH#1
| Cell ID: |  | -1

| Message Details:
| CMAC_Config_CNF:
cellId: | -1
| routingInfo:
physicalChannelIdentity: | 26

#### CPHY_RL_Setup_REQ

RRC |  | LLA | @ 00:00:10.240

| Channel ID: |  | UL-DPCH#1
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_REQ:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 20
ratType: | fdd
| setupMessage: (CphyRlSetupReq)
| physicalChannelInfo:
| dPCHInfo:
| ul_DPCHInfo: (UL_DPCH_Info)
| ul_DPCH_PowerControlInfo:
| fdd:
dpcch_PowerOffset: | -40
pc_Preamble: | 1
sRB_delay: | 7
| powerControlAlgorithm:
algorithm1 (TPC_StepSizeFDD): | 1
| modeSpecificInfo:
| fdd:
scramblingCodeType: | longSC
scramblingCode (UL_ScramblingCode): | 0
numberOfDPDCH: | Omit
spreadingFactor: | sf64
tfci_Existence: | true
numberOfFBI_Bits: | Omit
puncturingLimit: | pl1
| dl_DPCHInfo: Omit

#### CPHY_RL_Setup_CNF

LLA |  | RRC | @ 00:00:10.250

| Channel ID: |  | UL-DPCH#1
| Cell ID: |  | 0

| Message Details:
| CPHY_RL_Setup_CNF:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 20

#### CPHY_TrCH_Config_REQ

RRC |  | LLA | @ 00:00:10.250

| Channel ID: |  | UL-DPCH#1
| Cell ID: |  | 0

| Message Details:
| CPHY_TrCH_Config_REQ:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 20
ratType: | fdd
| trchConfigType:
dch: | Normal
| configMessage: (CphyTrchConfigReq)
| activationTime: (SS_ActivationTime)
activateNow: |
| ulconnectedTrCHList:
| :
trchid (TransportChannelIdentity): | 5
ul_TransportChannelType (SS_UL_TransportChannelType): | dch
| transportChannelInfo: (CommonOrDedicatedTFS)
| tti:
| tti10: (CommonOrDedicatedTF_InfoList)
| CommonOrDedicatedTF_Info:
tb_Size: | 148
| numberOfTbSizeList:
| NumberOfTransportBlocks:
zero: |
| NumberOfTransportBlocks:
one: |
| logicalChannelList:
allSizes: |
| semistaticTF_Information:
| channelCodingType:
convolutional (CodingRate): | third
rateMatchingAttribute: | 192
crc_Size: | crc16
| ulTFCS: (TFCS)
| normalTFCI_Signalling: (ExplicitTFCS_Configuration)
| complete: (TFCS_ReconfAdd)
| ctfcSize:
| ctfc2Bit:
| :
ctfc2: | 0
| powerOffsetInformation: Omit
| :
ctfc2: | 1
| powerOffsetInformation: Omit
| dlconnectedTrCHList: Omit
| dlTFCS: (TFCS) Omit

#### CPHY Radio Link Setup REQ

LLA |  | PHY | @ 00:00:10.310

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: U_DPCH
| CFN: |  | 16

| Message Details:
| Configuration Parameters:
Channel Offset: | 8704
Scrambling Code: | 16777216
Symbol Rate: | 60k
Channelization Code: | 0
Adjust Time: | 0
Slot Format: | 0
Number Of DPDCH: | 1
| DPDCH Parameters:
| Item Number 0:
Channelization Code: | 16

#### CPHY Radio Link Setup CNF

PHY |  | LLA | @ 00:00:10.310

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: U_DPCH
| CFN: |  | 16

| Message Details:

#### CPHY Transport Channel Configuration REQ

LLA |  | PHY | @ 00:00:10.570

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: U_DPCH
| CFN: |  | 42

| Message Details:
| Configuration Parameters:
DTX Position: | Flexible
Second Interleave: | On
Puncture Limit: | 100
CCTrCH Length: | 600
Number Of Transport Channels: | 1
| Transport Channels:
| Item Number 0:
| Transport Channel Parameters:
| Transport Channel:
Name: | U_DCH
Identity: | 0
TTI (ms): | 10
EP Type: | 1/3 Rate Convolutional Coding
CRC Size: | 16
RM Attribute: | 192
First Interleave: | On
Number Of Transport Formats: | 2
| Transport Format Set:
| Transport Format 0:
Number Of Transport Blocks: | 0
Transport Block Size In Bits: | 148
| Transport Format 1:
Number Of Transport Blocks: | 1
Transport Block Size In Bits: | 148
RM Maximum Length: | 600
| Transport Format Combination Set:
Number Of Transport Format Combinations: | 2
| Transport Format Combinations 0:
Transport Format: | 0
| Transport Format Combinations 1:
Transport Format: | 1

#### CPHY Transport Channel Configuration CNF

PHY |  | LLA | @ 00:00:10.590

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: U_DPCH
| CFN: |  | 44

| Message Details:

#### CPHY_TrCH_Config_CNF

LLA |  | RRC | @ 00:00:10.610

| Channel ID: |  | UL-DPCH#1
| Cell ID: |  | 0

| Message Details:
| CPHY_TrCH_Config_CNF:
cellId: | 0
| routingInfo:
physicalChannelIdentity: | 20

#### CMAC_Config_REQ

RRC |  | LLA | @ 00:00:10.610

| Channel ID: |  | UL-DPCH#1
| Cell ID: |  | -1

| Message Details:
| CMAC_Config_REQ:
cellId: | -1
| routingInfo:
physicalChannelIdentity: | 20
ratType: | fdd
| configMessage:
| setup: (CmacConfigReq)
| activationTime: (SS_ActivationTime)
activateNow: |
| uE_Info:
| u_RNTI: Omit
c_RNTI: | Omit
| trCHInfo:
| ulconnectedTrCHList:
| :
trchid (TransportChannelIdentity): | 5
| transportChannelInfo: (CommonOrDedicatedTFS)
| tti:
| tti10: (CommonOrDedicatedTF_InfoList)
| CommonOrDedicatedTF_Info:
tb_Size: | 148
| numberOfTbSizeList:
| NumberOfTransportBlocks:
zero: |
| NumberOfTransportBlocks:
one: |
| logicalChannelList:
allSizes: |
| semistaticTF_Information:
| channelCodingType:
convolutional (CodingRate): | third
rateMatchingAttribute: | 192
crc_Size: | crc16
| ulTFCS: (TFCS)
| normalTFCI_Signalling: (ExplicitTFCS_Configuration)
| complete: (TFCS_ReconfAdd)
| ctfcSize:
| ctfc2Bit:
| :
ctfc2: | 0
| powerOffsetInformation: Omit
| :
ctfc2: | 1
| powerOffsetInformation: Omit
| dlconnectedTrCHList: Omit
| dlTFCS: (TFCS) Omit
| trCH_LogCHMapping: (TrCH_LogCHMappingList1)
| ulconnectedTrCHList:
| :
trchid (TransportChannelIdentity): | 5
| trCH_LogCHMappingList:
| TrCH_LogicalChannelMapping:
| logicalChannel_Mapping:
| ul_LogicalChannelMapping: (SS_UL_LogicalChannelMapping)
macHeaderManipulation (MAC_HeaderManipulation): | normalMacHeader
ul_TransportChannelType (SS_UL_TransportChannelType): | dch
logicalChannelIdentity: | 1
logicalChannelType: | dCCH
rB_Identity: | 1
cn_DomainIdentity: | Omit
| TrCH_LogicalChannelMapping:
| logicalChannel_Mapping:
| ul_LogicalChannelMapping: (SS_UL_LogicalChannelMapping)
macHeaderManipulation (MAC_HeaderManipulation): | normalMacHeader
ul_TransportChannelType (SS_UL_TransportChannelType): | dch
logicalChannelIdentity: | 2
logicalChannelType: | dCCH
rB_Identity: | 2
cn_DomainIdentity: | Omit
| TrCH_LogicalChannelMapping:
| logicalChannel_Mapping:
| ul_LogicalChannelMapping: (SS_UL_LogicalChannelMapping)
macHeaderManipulation (MAC_HeaderManipulation): | normalMacHeader
ul_TransportChannelType (SS_UL_TransportChannelType): | dch
logicalChannelIdentity: | 3
logicalChannelType: | dCCH
rB_Identity: | 3
cn_DomainIdentity: | Omit
| TrCH_LogicalChannelMapping:
| logicalChannel_Mapping:
| ul_LogicalChannelMapping: (SS_UL_LogicalChannelMapping)
macHeaderManipulation (MAC_HeaderManipulation): | normalMacHeader
ul_TransportChannelType (SS_UL_TransportChannelType): | dch
logicalChannelIdentity: | 4
logicalChannelType: | dCCH
rB_Identity: | 4
cn_DomainIdentity: | Omit
| dlconnectedTrCHList: Omit

#### CMAC Configuration REQ

LLA |  | MAC | @ 00:00:10.630

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: U_DPCH
| CFN: |  | 48

| Message Details:
| Configuration Parameters:
Number Of Transport Channels: | 1
| Transport Channels:
| Item Number 0:
| Transport Channel Parameters:
| Transport Channel:
Name: | U_DCH
Identity: | 0
TTI (ms): | 10
EP Type: | 1/3 Rate Convolutional Coding
CRC Size: | 16
RM Attribute: | 192
First Interleave: | On
Number Of Transport Formats: | 2
| Transport Format Set:
| Transport Format 0:
Number Of Transport Blocks: | 0
Transport Block Size In Bits: | 148
| Transport Format 1:
Number Of Transport Blocks: | 1
Transport Block Size In Bits: | 148
Number Of Logical Channels: | 4
| Logical Channels:
| Item Number 0:
| Logical Channel:
Name: | DCCH
Identity: | 1
Priority: | 0
CT Length: | 4
CT Value: | 0
TCTF Length: | 0
TCTF Value: | 0
UE ID Type: | Not used
UE ID: | 0
| Item Number 1:
| Logical Channel:
Name: | DCCH
Identity: | 2
Priority: | 0
CT Length: | 4
CT Value: | 1
TCTF Length: | 0
TCTF Value: | 0
UE ID Type: | Not used
UE ID: | 0
| Item Number 2:
| Logical Channel:
Name: | DCCH
Identity: | 3
Priority: | 0
CT Length: | 4
CT Value: | 2
TCTF Length: | 0
TCTF Value: | 0
UE ID Type: | Not used
UE ID: | 0
| Item Number 3:
| Logical Channel:
Name: | DCCH
Identity: | 4
Priority: | 0
CT Length: | 4
CT Value: | 3
TCTF Length: | 0
TCTF Value: | 0
UE ID Type: | Not used
UE ID: | 0
Active Flag: | 1
| Transport Format Combination Set:
Number Of Transport Format Combinations: | 2
| Transport Format Combinations 0:
Transport Format: | 0
| Transport Format Combinations 1:
Transport Format: | 1

#### CMAC Configuration CNF

MAC |  | LLA | @ 00:00:10.630

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: U_DPCH
| CFN: |  | 48

| Message Details:

#### CMAC_Config_CNF

LLA |  | RRC | @ 00:00:10.650

| Channel ID: |  | UL-DPCH#1
| Cell ID: |  | -1

| Message Details:
| CMAC_Config_CNF:
cellId: | -1
| routingInfo:
physicalChannelIdentity: | 20

#### CRLC_Config_REQ

RRC |  | LLA | @ 00:00:10.650

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CRLC_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CrlcConfigReq)
| setup: (RBInfo)
| sS_rlc_Info:
| sS_ul_RLC_Mode: (DL_RLC_Mode) Omit
| sS_dl_RLC_Mode:
dl_PayloadSize (PayloadSize): | 246
| dl_RLCModeInfo: (UL_RLC_Mode)
| ul_TM_RLC_Mode:
| transmissionRLC_Discard: Omit
segmentationIndication: | false
| rB_LogCH_Mapping:
uLlogicalChannelIdentity (LogicalChannelIdentity): | Omit
dLlogicalChannelIdentity (LogicalChannelIdentity): | 1
logicalChannelType: | Omit
cn_DomainIdentity: | Omit

#### CRLC TM Channel Establish REQ

LLA |  | RLC | @ 00:00:10.790

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCCH
| CFN: |  | 64

| Message Details:
| Configuration Parameters:
Number Of PU Sizes: | 1
| PU sizes In Bits:
Item 0: | 246

#### CRLC TM Channel Establish CNF

RLC |  | LLA | @ 00:00:10.790

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCCH
| CFN: |  | 64

| Message Details:

#### CRLC_Config_CNF

LLA |  | RRC | @ 00:00:10.820

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CRLC_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### CRLC_Config_REQ

RRC |  | LLA | @ 00:00:10.820

| Channel ID: |  | RbPcch
| Cell ID: |  | 0

| Message Details:
| CRLC_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -2
ratType: | fdd
| configMessage: (CrlcConfigReq)
| setup: (RBInfo)
| sS_rlc_Info:
| sS_ul_RLC_Mode: (DL_RLC_Mode) Omit
| sS_dl_RLC_Mode:
dl_PayloadSize (PayloadSize): | 240
| dl_RLCModeInfo: (UL_RLC_Mode)
| ul_TM_RLC_Mode:
| transmissionRLC_Discard: Omit
segmentationIndication: | false
| rB_LogCH_Mapping:
uLlogicalChannelIdentity (LogicalChannelIdentity): | Omit
dLlogicalChannelIdentity (LogicalChannelIdentity): | 1
logicalChannelType: | Omit
cn_DomainIdentity: | Omit

#### CRLC TM Channel Establish REQ

LLA |  | RLC | @ 00:00:10.950

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: PCCH
| CFN: |  | 80

| Message Details:
| Configuration Parameters:
Number Of PU Sizes: | 1
| PU sizes In Bits:
Item 0: | 240

#### CRLC TM Channel Establish CNF

RLC |  | LLA | @ 00:00:10.950

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: PCCH
| CFN: |  | 80

| Message Details:

#### CRLC_Config_CNF

LLA |  | RRC | @ 00:00:10.960

| Channel ID: |  | RbPcch
| Cell ID: |  | 0

| Message Details:
| CRLC_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -2

#### CRLC_Config_REQ

RRC |  | LLA | @ 00:00:10.960

| Channel ID: |  | Rb0
| Cell ID: |  | 0

| Message Details:
| CRLC_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | 0
ratType: | fdd
| configMessage: (CrlcConfigReq)
| setup: (RBInfo)
| sS_rlc_Info:
| sS_ul_RLC_Mode: (DL_RLC_Mode) Omit
| sS_dl_RLC_Mode:
dl_PayloadSize (PayloadSize): | 152
| dl_RLCModeInfo: (UL_RLC_Mode)
| ul_UM_RLC_Mode:
| transmissionRLC_Discard:
timerBasedNoExplicit (NoExplicitDiscard): | dt100
| rB_LogCH_Mapping:
uLlogicalChannelIdentity (LogicalChannelIdentity): | Omit
dLlogicalChannelIdentity (LogicalChannelIdentity): | 5
logicalChannelType: | Omit
cn_DomainIdentity: | Omit

#### CRLC UM Channel Establish REQ

LLA |  | RLC | @ 00:00:11.060

| BTS unit: |  | 1:1
| Channel No: |  | 1 Name: CCCH
| CFN: |  | 91

| Message Details:
| Configuration Parameters:
PU Size In Bits: | 152

#### CRLC UM Channel Establish CNF

RLC |  | LLA | @ 00:00:11.060

| BTS unit: |  | 1:1
| Channel No: |  | 1 Name: CCCH
| CFN: |  | 91

| Message Details:

#### CRLC_Config_CNF

LLA |  | RRC | @ 00:00:11.070

| Channel ID: |  | Rb0
| Cell ID: |  | 0

| Message Details:
| CRLC_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | 0

#### CRLC_Config_REQ

RRC |  | LLA | @ 00:00:11.070

| Channel ID: |  | Rb0
| Cell ID: |  | 0

| Message Details:
| CRLC_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | 0
ratType: | fdd
| configMessage: (CrlcConfigReq)
| setup: (RBInfo)
| sS_rlc_Info:
| sS_ul_RLC_Mode: (DL_RLC_Mode)
| dl_TM_RLC_Mode:
segmentationIndication: | false
| sS_dl_RLC_Mode:
dl_PayloadSize (PayloadSize): | 166
| dl_RLCModeInfo: (UL_RLC_Mode)
| ul_TM_RLC_Mode:
| transmissionRLC_Discard: Omit
segmentationIndication: | false
| rB_LogCH_Mapping:
uLlogicalChannelIdentity (LogicalChannelIdentity): | 5
dLlogicalChannelIdentity (LogicalChannelIdentity): | Omit
logicalChannelType: | Omit
cn_DomainIdentity: | Omit

#### CRLC TM Channel Establish REQ

LLA |  | RLC | @ 00:00:11.110

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: CCCH
| CFN: |  | 96

| Message Details:
| Configuration Parameters:
Number Of PU Sizes: | 1
| PU sizes In Bits:
Item 0: | 166

#### CRLC TM Channel Establish CNF

RLC |  | LLA | @ 00:00:11.110

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: CCCH
| CFN: |  | 96

| Message Details:

#### CRLC_Config_CNF

LLA |  | RRC | @ 00:00:11.130

| Channel ID: |  | Rb0
| Cell ID: |  | 0

| Message Details:
| CRLC_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | 0

#### CRLC_Config_REQ

RRC |  | LLA | @ 00:00:11.130

| Channel ID: |  | Rb1
| Cell ID: |  | -1

| Message Details:
| CRLC_Config_REQ:
cellId: | -1
| routingInfo:
rB_Identity: | 1
ratType: | fdd
| configMessage: (CrlcConfigReq)
| setup: (RBInfo)
| sS_rlc_Info:
| sS_ul_RLC_Mode: (DL_RLC_Mode)
dl_UM_RLC_Mode: |
| sS_dl_RLC_Mode:
dl_PayloadSize (PayloadSize): | 136
| dl_RLCModeInfo: (UL_RLC_Mode)
| ul_UM_RLC_Mode:
| transmissionRLC_Discard:
timerBasedNoExplicit (NoExplicitDiscard): | dt100
| rB_LogCH_Mapping:
uLlogicalChannelIdentity (LogicalChannelIdentity): | 1
dLlogicalChannelIdentity (LogicalChannelIdentity): | 1
logicalChannelType: | Omit
cn_DomainIdentity: | Omit

#### CRLC UM Channel Establish REQ

LLA |  | RLC | @ 00:00:11.270

| BTS unit: |  | 1:1
| Channel No: |  | 1 Name: DCCH
| CFN: |  | 112

| Message Details:
| Configuration Parameters:
PU Size In Bits: | 136

#### CRLC UM Channel Establish CNF

RLC |  | LLA | @ 00:00:11.270

| BTS unit: |  | 1:1
| Channel No: |  | 1 Name: DCCH
| CFN: |  | 112

| Message Details:

#### CRLC_Config_CNF

LLA |  | RRC | @ 00:00:11.300

| Channel ID: |  | Rb1
| Cell ID: |  | -1

| Message Details:
| CRLC_Config_CNF:
cellId: | -1
| routingInfo:
rB_Identity: | 1

#### CRLC_Config_REQ

RRC |  | LLA | @ 00:00:11.300

| Channel ID: |  | Rb2
| Cell ID: |  | -1

| Message Details:
| CRLC_Config_REQ:
cellId: | -1
| routingInfo:
rB_Identity: | 2
ratType: | fdd
| configMessage: (CrlcConfigReq)
| setup: (RBInfo)
| sS_rlc_Info:
| sS_ul_RLC_Mode: (DL_RLC_Mode)
| dl_AM_RLC_Mode:
inSequenceDelivery: | true
receivingWindowSize: | rw32
| dl_RLC_StatusInfo:
timerStatusProhibit: | tsp200
timerEPC: | Omit
missingPDU_Indicator: | true
timerStatusPeriodic: | Omit
| sS_dl_RLC_Mode:
dl_PayloadSize (PayloadSize): | 128
| dl_RLCModeInfo: (UL_RLC_Mode)
| ul_AM_RLC_Mode:
| transmissionRLC_Discard:
noDiscard (MaxDAT): | dat15
transmissionWindowSize: | tw32
timerRST: | tr500
max_RST (MaxRST): | rst1
| pollingInfo:
timerPollProhibit: | tpp200
timerPoll: | tp200
poll_PDU: | Omit
poll_SDU: | sdu1
lastTransmissionPDU_Poll: | true
lastRetransmissionPDU_Poll: | true
pollWindow: | pw99
timerPollPeriodic: | Omit
| rB_LogCH_Mapping:
uLlogicalChannelIdentity (LogicalChannelIdentity): | 2
dLlogicalChannelIdentity (LogicalChannelIdentity): | 2
logicalChannelType: | Omit
cn_DomainIdentity: | Omit

#### CRLC AM Channel Establish REQ

LLA |  | RLC | @ 00:00:11.430

| BTS unit: |  | 1:1
| Channel No: |  | 2 Name: DCCH
| CFN: |  | 128

| Message Details:
| Configuration Parameters:
PU Size In Bits: | 128
| Timer Parameters:
Poll (ms): | 200
Poll Prohibit (ms): | 0
EPC (ms): | 0
Discard (ms): | 0
Poll Periodic (ms): | 0
Status Prohibit (ms): | 0
Status Periodic (ms): | 0
Reset (ms): | 500
MRW (ms): | 0
| Protocol Parameters:
Max Dat: | 15
Poll PU: | 0
Poll SDU: | 1
Poll Window: | 99
Max Reset: | 1
Tx Window Size: | 32
Rx Window Size: | 32
Max MRW: | 0
SDU Discard Mode: | No discard
| Polling Triggers:
Last PU In Buffer: | On
Last PU In Retransmission Buffer: | On
Poll Timer: | On
Every Poll-PU PU: | Off
Every Poll-SDU SDU: | On
Poll-Window Percent Of Transmission Buffer: | On
Timer Based: | Off
| Status Triggers:
Missing PU: | On
Timer Based: | Off
EPC Mechanism: | Off

#### CRLC AM Channel Establish CNF

RLC |  | LLA | @ 00:00:11.430

| BTS unit: |  | 1:1
| Channel No: |  | 2 Name: DCCH
| CFN: |  | 128

| Message Details:

#### CRLC_Config_CNF

LLA |  | RRC | @ 00:00:11.440

| Channel ID: |  | Rb2
| Cell ID: |  | -1

| Message Details:
| CRLC_Config_CNF:
cellId: | -1
| routingInfo:
rB_Identity: | 2

#### CRLC_Config_REQ

RRC |  | LLA | @ 00:00:11.440

| Channel ID: |  | Rb3
| Cell ID: |  | -1

| Message Details:
| CRLC_Config_REQ:
cellId: | -1
| routingInfo:
rB_Identity: | 3
ratType: | fdd
| configMessage: (CrlcConfigReq)
| setup: (RBInfo)
| sS_rlc_Info:
| sS_ul_RLC_Mode: (DL_RLC_Mode)
| dl_AM_RLC_Mode:
inSequenceDelivery: | true
receivingWindowSize: | rw32
| dl_RLC_StatusInfo:
timerStatusProhibit: | tsp200
timerEPC: | Omit
missingPDU_Indicator: | true
timerStatusPeriodic: | Omit
| sS_dl_RLC_Mode:
dl_PayloadSize (PayloadSize): | 128
| dl_RLCModeInfo: (UL_RLC_Mode)
| ul_AM_RLC_Mode:
| transmissionRLC_Discard:
noDiscard (MaxDAT): | dat15
transmissionWindowSize: | tw32
timerRST: | tr500
max_RST (MaxRST): | rst1
| pollingInfo:
timerPollProhibit: | tpp200
timerPoll: | tp200
poll_PDU: | Omit
poll_SDU: | sdu1
lastTransmissionPDU_Poll: | true
lastRetransmissionPDU_Poll: | true
pollWindow: | pw99
timerPollPeriodic: | Omit
| rB_LogCH_Mapping:
uLlogicalChannelIdentity (LogicalChannelIdentity): | 3
dLlogicalChannelIdentity (LogicalChannelIdentity): | 3
logicalChannelType: | Omit
cn_DomainIdentity: | Omit

#### CRLC AM Channel Establish REQ

LLA |  | RLC | @ 00:00:11.480

| BTS unit: |  | 1:1
| Channel No: |  | 3 Name: DCCH
| CFN: |  | 133

| Message Details:
| Configuration Parameters:
PU Size In Bits: | 128
| Timer Parameters:
Poll (ms): | 200
Poll Prohibit (ms): | 0
EPC (ms): | 0
Discard (ms): | 0
Poll Periodic (ms): | 0
Status Prohibit (ms): | 0
Status Periodic (ms): | 0
Reset (ms): | 500
MRW (ms): | 0
| Protocol Parameters:
Max Dat: | 15
Poll PU: | 0
Poll SDU: | 1
Poll Window: | 99
Max Reset: | 1
Tx Window Size: | 32
Rx Window Size: | 32
Max MRW: | 0
SDU Discard Mode: | No discard
| Polling Triggers:
Last PU In Buffer: | On
Last PU In Retransmission Buffer: | On
Poll Timer: | On
Every Poll-PU PU: | Off
Every Poll-SDU SDU: | On
Poll-Window Percent Of Transmission Buffer: | On
Timer Based: | Off
| Status Triggers:
Missing PU: | On
Timer Based: | Off
EPC Mechanism: | Off

#### CRLC AM Channel Establish CNF

RLC |  | LLA | @ 00:00:11.480

| BTS unit: |  | 1:1
| Channel No: |  | 3 Name: DCCH
| CFN: |  | 133

| Message Details:

#### CRLC_Config_CNF

LLA |  | RRC | @ 00:00:11.490

| Channel ID: |  | Rb3
| Cell ID: |  | -1

| Message Details:
| CRLC_Config_CNF:
cellId: | -1
| routingInfo:
rB_Identity: | 3

#### CRLC_Config_REQ

RRC |  | LLA | @ 00:00:11.490

| Channel ID: |  | Rb4
| Cell ID: |  | -1

| Message Details:
| CRLC_Config_REQ:
cellId: | -1
| routingInfo:
rB_Identity: | 4
ratType: | fdd
| configMessage: (CrlcConfigReq)
| setup: (RBInfo)
| sS_rlc_Info:
| sS_ul_RLC_Mode: (DL_RLC_Mode)
| dl_AM_RLC_Mode:
inSequenceDelivery: | true
receivingWindowSize: | rw32
| dl_RLC_StatusInfo:
timerStatusProhibit: | tsp200
timerEPC: | Omit
missingPDU_Indicator: | true
timerStatusPeriodic: | Omit
| sS_dl_RLC_Mode:
dl_PayloadSize (PayloadSize): | 128
| dl_RLCModeInfo: (UL_RLC_Mode)
| ul_AM_RLC_Mode:
| transmissionRLC_Discard:
noDiscard (MaxDAT): | dat15
transmissionWindowSize: | tw32
timerRST: | tr500
max_RST (MaxRST): | rst1
| pollingInfo:
timerPollProhibit: | tpp200
timerPoll: | tp200
poll_PDU: | Omit
poll_SDU: | sdu1
lastTransmissionPDU_Poll: | true
lastRetransmissionPDU_Poll: | true
pollWindow: | pw99
timerPollPeriodic: | Omit
| rB_LogCH_Mapping:
uLlogicalChannelIdentity (LogicalChannelIdentity): | 4
dLlogicalChannelIdentity (LogicalChannelIdentity): | 4
logicalChannelType: | Omit
cn_DomainIdentity: | Omit

#### CRLC AM Channel Establish REQ

LLA |  | RLC | @ 00:00:11.590

| BTS unit: |  | 1:1
| Channel No: |  | 4 Name: DCCH
| CFN: |  | 144

| Message Details:
| Configuration Parameters:
PU Size In Bits: | 128
| Timer Parameters:
Poll (ms): | 200
Poll Prohibit (ms): | 0
EPC (ms): | 0
Discard (ms): | 0
Poll Periodic (ms): | 0
Status Prohibit (ms): | 0
Status Periodic (ms): | 0
Reset (ms): | 500
MRW (ms): | 0
| Protocol Parameters:
Max Dat: | 15
Poll PU: | 0
Poll SDU: | 1
Poll Window: | 99
Max Reset: | 1
Tx Window Size: | 32
Rx Window Size: | 32
Max MRW: | 0
SDU Discard Mode: | No discard
| Polling Triggers:
Last PU In Buffer: | On
Last PU In Retransmission Buffer: | On
Poll Timer: | On
Every Poll-PU PU: | Off
Every Poll-SDU SDU: | On
Poll-Window Percent Of Transmission Buffer: | On
Timer Based: | Off
| Status Triggers:
Missing PU: | On
Timer Based: | Off
EPC Mechanism: | Off

#### CRLC AM Channel Establish CNF

RLC |  | LLA | @ 00:00:11.590

| BTS unit: |  | 1:1
| Channel No: |  | 4 Name: DCCH
| CFN: |  | 144

| Message Details:

#### CRLC_Config_CNF

LLA |  | RRC | @ 00:00:11.600

| Channel ID: |  | Rb4
| Cell ID: |  | -1

| Message Details:
| CRLC_Config_CNF:
cellId: | -1
| routingInfo:
rB_Identity: | 4

#### o_SIB_PER_Encoding

RRC |  | RRC | @ 00:00:11.610

| Category: |  | TSO

| Message Details:
| Inputs:
| SIB:
| sIB1: (SysInfoType1)
cn_CommonGSM_MAP_NAS_SysInfo (NAS_SystemInformationGSM_MAP): |
[0] | 00 | 01 |  |  |  |  |  |
| cn_DomainSysInfoList:
| CN_DomainSysInfo:
cn_DomainIdentity: | ps_domain
| cn_Type:
gsm_MAP (NAS_SystemInformationGSM_MAP): |
[0] | 05 | 00 |  |  |  |  |  |
cn_DRX_CycleLengthCoeff (CN_DRX_CycleLengthCoefficient): | 7
| CN_DomainSysInfo:
cn_DomainIdentity: | cs_domain
| cn_Type:
gsm_MAP (NAS_SystemInformationGSM_MAP): |
[0] | 1E | 01 |  |  |  |  |  |
cn_DRX_CycleLengthCoeff (CN_DRX_CycleLengthCoefficient): | 7
| ue_ConnTimersAndConstants:
t_301: | Omit
n_301: | Omit
t_302: | Omit
n_302: | Omit
t_304: | Omit
n_304: | Omit
t_305: | Omit
t_307: | Omit
t_308: | Omit
t_309: | Omit
t_310: | Omit
n_310: | Omit
t_311: | Omit
t_312: | Omit
n_312: | Omit
t_313: | Omit
n_313: | Omit
t_314: | Omit
t_315: | Omit
n_315: | Omit
t_316: | Omit
t_317: | Omit
| ue_IdleTimersAndConstants:
t_300: | ms4000
n_300: | 3
t_312: | 10
n_312: | s1
| v3a0NonCriticalExtensions: Omit
| Outputs:
BITSTRING: |
[0] | 11 | 00 | 01 | 00 | 00 | 00 | 00 | 00
[8] | 00 | 00 | 01 | 01 | 10 | 00 | 10 | 00
[16] | 00 | 10 | 10 | 00 | 00 | 00 | 00 | 10
[24] | 00 | 01 | 00 | 01 | 11 | 10 | 00 | 00
[32] | 00 | 01 | 01 | 00 | 00 | 00 | 00 | 00
[40] | 00 | 00 | 00 | 00 | 00 | 00 | 11 | 00
[48] | 01 | 11 | 01 | 00 | 00 |  |  |

#### o_SIB_PER_Encoding

RRC |  | RRC | @ 00:00:11.610

| Category: |  | TSO

| Message Details:
| Inputs:
| SIB:
| sIB2: (SysInfoType2)
| ura_IdentityList:
URA_Identity: | 0000000000000001
| nonCriticalExtensions: Omit
| Outputs:
BITSTRING: |
[0] | 00 | 00 | 00 | 00 | 00 | 00 | 00 | 00
[8] | 00 | 01 |  |  |  |  |  |

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:11.610

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 10
bcch_ModificationTime: | Omit

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:11.630

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:11.630

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
| completeSIB_List:
| CompleteSIBshort:
sib_Type: | systemInformationBlockType1
sib_Data_variable: | 1100010000000000000001011000100000101000000000100001000111100000000101000000000000000000000011000111010000
| CompleteSIBshort:
sib_Type: | systemInformationBlockType2
sib_Data_variable: | 00000000000000000001

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA |  | RLC | @ 00:00:11.650

| Channel No: |  | 0 Name: BCCH

| Message Details:
| SIB repetition rate: 64
| SIB position: 20
| BCCH_BCH_Message:
| message:
| sfn_Prime: 0
| payload:
| completeSIB_List:
| CompleteSIB_List.element:
| sib_Type: systemInformationBlockType1_SIB_Type [enum=1]
| sib_Data_variable: 1100010000000000000001011000100000101000000000100001000111100000000101000000000000000000000011000111010000
| CompleteSIB_List.element:
| sib_Type: systemInformationBlockType2_SIB_Type [enum=2]
| sib_Data_variable: 00000000000000000001
Layer 3 SDU: |
[0] | 00 | 0E | 21 | 69 | C4 | 00 | 05 | 88
[8] | 28 | 02 | 11 | E0 | 14 | 00 | 00 | 0C
[16] | 74 | 04 | 26 | 00 | 00 | 20 |  |

#### o_SIB_PER_Encoding

RRC |  | RRC | @ 00:00:11.650

| Category: |  | TSO

| Message Details:
| Inputs:
| SIB:
| sIB2: (SysInfoType2)
| ura_IdentityList:
URA_Identity: | 0000000000000001
| nonCriticalExtensions: Omit
| Outputs:
BITSTRING: |
[0] | 00 | 00 | 00 | 00 | 00 | 00 | 00 | 00
[8] | 00 | 01 |  |  |  |  |  |

#### o_SIB_PER_Encoding

RRC |  | RRC | @ 00:00:11.660

| Category: |  | TSO

| Message Details:
| Inputs:
| SIB:
| sIB1: (SysInfoType1)
cn_CommonGSM_MAP_NAS_SysInfo (NAS_SystemInformationGSM_MAP): |
[0] | 00 | 01 |  |  |  |  |  |
| cn_DomainSysInfoList:
| CN_DomainSysInfo:
cn_DomainIdentity: | ps_domain
| cn_Type:
gsm_MAP (NAS_SystemInformationGSM_MAP): |
[0] | 05 | 00 |  |  |  |  |  |
cn_DRX_CycleLengthCoeff (CN_DRX_CycleLengthCoefficient): | 7
| CN_DomainSysInfo:
cn_DomainIdentity: | cs_domain
| cn_Type:
gsm_MAP (NAS_SystemInformationGSM_MAP): |
[0] | 1E | 01 |  |  |  |  |  |
cn_DRX_CycleLengthCoeff (CN_DRX_CycleLengthCoefficient): | 7
| ue_ConnTimersAndConstants:
t_301: | Omit
n_301: | Omit
t_302: | Omit
n_302: | Omit
t_304: | Omit
n_304: | Omit
t_305: | Omit
t_307: | Omit
t_308: | Omit
t_309: | Omit
t_310: | Omit
n_310: | Omit
t_311: | Omit
t_312: | Omit
n_312: | Omit
t_313: | Omit
n_313: | Omit
t_314: | Omit
t_315: | Omit
n_315: | Omit
t_316: | Omit
t_317: | Omit
| ue_IdleTimersAndConstants:
t_300: | ms4000
n_300: | 3
t_312: | 10
n_312: | s1
| v3a0NonCriticalExtensions: Omit
| Outputs:
BITSTRING: |
[0] | 11 | 00 | 01 | 00 | 00 | 00 | 00 | 00
[8] | 00 | 00 | 01 | 01 | 10 | 00 | 10 | 00
[16] | 00 | 10 | 10 | 00 | 00 | 00 | 00 | 10
[24] | 00 | 01 | 00 | 01 | 11 | 10 | 00 | 00
[32] | 00 | 01 | 01 | 00 | 00 | 00 | 00 | 00
[40] | 00 | 00 | 00 | 00 | 00 | 00 | 11 | 00
[48] | 01 | 11 | 01 | 00 | 00 |  |  |

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:11.660

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 10
bcch_ModificationTime: | Omit

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:11.680

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:11.680

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
| completeSIB_List:
| CompleteSIBshort:
sib_Type: | systemInformationBlockType1
sib_Data_variable: | 1100010000000000000001011000100000101000000000100001000111100000000101000000000000000000000011000111010000
| CompleteSIBshort:
sib_Type: | systemInformationBlockType2
sib_Data_variable: | 00000000000000000001

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA |  | RLC | @ 00:00:11.680

| Channel No: |  | 0 Name: BCCH

| Message Details:
| SIB repetition rate: 64
| SIB position: 20
| BCCH_BCH_Message:
| message:
| sfn_Prime: 0
| payload:
| completeSIB_List:
| CompleteSIB_List.element:
| sib_Type: systemInformationBlockType1_SIB_Type [enum=1]
| sib_Data_variable: 1100010000000000000001011000100000101000000000100001000111100000000101000000000000000000000011000111010000
| CompleteSIB_List.element:
| sib_Type: systemInformationBlockType2_SIB_Type [enum=2]
| sib_Data_variable: 00000000000000000001
Layer 3 SDU: |
[0] | 00 | 0E | 21 | 69 | C4 | 00 | 05 | 88
[8] | 28 | 02 | 11 | E0 | 14 | 00 | 00 | 0C
[16] | 74 | 04 | 26 | 00 | 00 | 20 |  |

#### o_SIB_PER_Encoding

RRC |  | RRC | @ 00:00:11.680

| Category: |  | TSO

| Message Details:
| Inputs:
| SIB:
| sIB3: (SysInfoType3)
sib4indicator: | true
cellIdentity: | 0000000000000000000000000000
| cellSelectReselectInfo: (CellSelectReselectInfoSIB_3_4)
| mappingInfo: Omit
| cellSelectQualityMeasure:
cpich_RSCP: |
| modeSpecificInfo:
| fdd:
s_Intrasearch (S_SearchQual): | 8
s_Intersearch (S_SearchQual): | 8
s_SearchHCS (S_SearchRXLEV): | Omit
| rat_List: (RAT_FDD_InfoList)
| RAT_FDD_Info:
rat_Identifier: | gsm
s_SearchRAT (S_SearchQual): | -16
s_HCS_RAT (S_SearchRXLEV): | Omit
s_Limit_SearchRAT (S_SearchQual): | 0
q_QualMin: | -24
q_RxlevMin: | -40
q_Hyst_l_S (Q_Hyst_S): | 2
t_Reselection_S: | 0
| hcs_ServingCellInformation: Omit
maxAllowedUL_TX_Power: | 21
| cellAccessRestriction:
| cellBarred:
notBarred: |
cellReservedForOperatorUse (ReservedIndicator): | notReserved
cellReservationExtension (ReservedIndicator): | notReserved
| accessClassBarredList:
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
| nonCriticalExtensions: Omit
| Outputs:
BITSTRING: |
[0] | 01 | 00 | 00 | 00 | 00 | 00 | 00 | 00
[8] | 00 | 00 | 00 | 00 | 00 | 00 | 00 | 00
[16] | 10 | 11 | 01 | 11 | 00 | 01 | 10 | 00
[24] | 00 | 00 | 00 | 00 | 00 | 01 | 00 | 00
[32] | 00 | 00 | 00 | 10 | 01 | 00 | 00 | 10
[40] | 00 | 00 | 01 | 00 | 01 | 11 | 11 | 11
[48] | 11 | 11 | 11 | 11 | 11 | 11 | 11 | 11

#### o_SIB_PER_Encoding

RRC |  | RRC | @ 00:00:11.680

| Category: |  | TSO

| Message Details:
| Inputs:
| SIB:
| sIB7: (SysInfoType7)
| modeSpecificInfo:
| fdd:
ul_Interference: | -100
| prach_Information_SIB5_List: (DynamicPersistenceLevelList)
DynamicPersistenceLevel: | 2
| prach_Information_SIB6_List: (DynamicPersistenceLevelList)
DynamicPersistenceLevel: | 2
expirationTimeFactor: | Omit
| nonCriticalExtensions: Omit
| Outputs:
BITSTRING: |
[0] | 10 | 00 | 00 | 10 | 10 | 00 | 00 | 00
[8] | 10 | 00 | 00 | 01 |  |  |  |

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:11.680

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 7
bcch_ModificationTime: | Omit

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:11.690

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:11.690

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
| completeSIB_List:
| CompleteSIBshort:
sib_Type: | systemInformationBlockType7
sib_Data_variable: | 100000101000000010000001
| CompleteSIBshort:
sib_Type: | systemInformationBlockType3
sib_Data_variable: | 0100000000000000000000000000000010110111000110000000000000010000000000100100001000000100011111111111111111111111

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA |  | RLC | @ 00:00:11.690

| Channel No: |  | 0 Name: BCCH

| Message Details:
| SIB repetition rate: 64
| SIB position: 14
| BCCH_BCH_Message:
| message:
| sfn_Prime: 0
| payload:
| completeSIB_List:
| CompleteSIB_List.element:
| sib_Type: systemInformationBlockType7_SIB_Type [enum=7]
| sib_Data_variable: 100000101000000010000001
| CompleteSIB_List.element:
| sib_Type: systemInformationBlockType3_SIB_Type [enum=3]
| sib_Data_variable: 0100000000000000000000000000000010110111000110000000000000010000000000100100001000000100011111111111111111111111
Layer 3 SDU: |
[0] | 00 | 0E | 27 | 17 | 82 | 80 | 81 | 1B
[8] | 7A | 00 | 00 | 00 | 05 | B8 | C0 | 00
[16] | 80 | 12 | 10 | 23 | FF | FF | F8 |

#### o_SIB_PER_Encoding

RRC |  | RRC | @ 00:00:11.690

| Category: |  | TSO

| Message Details:
| Inputs:
| SIB:
| sIB4: (SysInfoType4)
cellIdentity: | 0000000000000000000000000000
| cellSelectReselectInfo: (CellSelectReselectInfoSIB_3_4)
| mappingInfo: Omit
| cellSelectQualityMeasure:
cpich_RSCP: |
| modeSpecificInfo:
| fdd:
s_Intrasearch (S_SearchQual): | 8
s_Intersearch (S_SearchQual): | 8
s_SearchHCS (S_SearchRXLEV): | Omit
| rat_List: (RAT_FDD_InfoList)
| RAT_FDD_Info:
rat_Identifier: | gsm
s_SearchRAT (S_SearchQual): | -16
s_HCS_RAT (S_SearchRXLEV): | Omit
s_Limit_SearchRAT (S_SearchQual): | 0
q_QualMin: | -24
q_RxlevMin: | -40
q_Hyst_l_S (Q_Hyst_S): | 0
t_Reselection_S: | 0
| hcs_ServingCellInformation: Omit
maxAllowedUL_TX_Power: | 21
| cellAccessRestriction:
| cellBarred:
notBarred: |
cellReservedForOperatorUse (ReservedIndicator): | notReserved
cellReservationExtension (ReservedIndicator): | notReserved
| accessClassBarredList: Omit
| nonCriticalExtensions: Omit
| Outputs:
BITSTRING: |
[0] | 00 | 00 | 00 | 00 | 00 | 00 | 00 | 00
[8] | 00 | 00 | 00 | 00 | 00 | 00 | 00 | 01
[16] | 01 | 10 | 11 | 10 | 00 | 11 | 00 | 00
[24] | 00 | 00 | 00 | 00 | 00 | 10 | 00 | 00
[32] | 00 | 00 | 01 | 00 | 10 | 00 | 00 | 00
[40] | 00 | 00 | 10 | 00 | 11 | 10 | 11 | 1

#### o_SIB_PER_Encoding

RRC |  | RRC | @ 00:00:11.690

| Category: |  | TSO

| Message Details:
| Inputs:
| SIB:
| sIB7: (SysInfoType7)
| modeSpecificInfo:
| fdd:
ul_Interference: | -100
| prach_Information_SIB5_List: (DynamicPersistenceLevelList)
DynamicPersistenceLevel: | 2
| prach_Information_SIB6_List: (DynamicPersistenceLevelList)
DynamicPersistenceLevel: | 2
expirationTimeFactor: | Omit
| nonCriticalExtensions: Omit
| Outputs:
BITSTRING: |
[0] | 10 | 00 | 00 | 10 | 10 | 00 | 00 | 00
[8] | 10 | 00 | 00 | 01 |  |  |  |

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:11.690

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 31
bcch_ModificationTime: | Omit

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:11.710

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:11.710

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
| completeSIB_List:
| CompleteSIBshort:
sib_Type: | systemInformationBlockType7
sib_Data_variable: | 100000101000000010000001
| CompleteSIBshort:
sib_Type: | systemInformationBlockType4
sib_Data_variable: | 00000000000000000000000000000001011011100011000000000000001000000000010010000000000010001110111

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA |  | RLC | @ 00:00:11.710

| Channel No: |  | 0 Name: BCCH

| Message Details:
| SIB repetition rate: 64
| SIB position: 62
| BCCH_BCH_Message:
| message:
| sfn_Prime: 0
| payload:
| completeSIB_List:
| CompleteSIB_List.element:
| sib_Type: systemInformationBlockType7_SIB_Type [enum=7]
| sib_Data_variable: 100000101000000010000001
| CompleteSIB_List.element:
| sib_Type: systemInformationBlockType4_SIB_Type [enum=4]
| sib_Data_variable: 00000000000000000000000000000001011011100011000000000000001000000000010010000000000010001110111
Layer 3 SDU: |
[0] | 00 | 0E | 27 | 17 | 82 | 80 | 81 | 22
[8] | F0 | 00 | 00 | 00 | 0B | 71 | 80 | 01
[16] | 00 | 24 | 00 | 47 | 70 |  |  |

#### o_SIB_PER_Encoding

RRC |  | RRC | @ 00:00:11.710

| Category: |  | TSO

| Message Details:
| Inputs:
| SIB:
| sIB5: (SysInfoType5)
sib6indicator: | true
pich_PowerOffset: | -5
| modeSpecificInfo:
| fdd:
aich_PowerOffset: | -5
| primaryCCPCH_Info: Omit
| prach_SystemInformationList:
| PRACH_SystemInformation:
| prach_RACH_Info:
| modeSpecificInfo:
| fdd:
availableSignatures: | 0000000011111111
availableSF (SF_PRACH): | sfpr64
preambleScramblingCodeWordNumber: | 0
puncturingLimit: | pl1
availableSubChannelNumbers: | 111111111111
transportChannelIdentity: | 15
| rach_TransportFormatSet: (TransportFormatSet)
| commonTransChTFS:
| tti:
| tti20: (CommonDynamicTF_InfoList)
| CommonDynamicTF_Info:
| rlc_Size:
| fdd:
| octetModeRLC_SizeInfoType2:
sizeType1: | 15
| numberOfTbSizeList:
| NumberOfTransportBlocks:
one: |
| logicalChannelList:
configured: |
| CommonDynamicTF_Info:
| rlc_Size:
| fdd:
| octetModeRLC_SizeInfoType2:
sizeType2: | 3
| numberOfTbSizeList:
| NumberOfTransportBlocks:
one: |
| logicalChannelList:
configured: |
| semistaticTF_Information:
| channelCodingType:
convolutional (CodingRate): | half
rateMatchingAttribute: | 150
crc_Size: | crc16
| rach_TFCS: (TFCS)
| normalTFCI_Signalling: (ExplicitTFCS_Configuration)
| complete: (TFCS_ReconfAdd)
| ctfcSize:
| ctfc2Bit:
| :
ctfc2: | 0
| powerOffsetInformation:
| gainFactorInformation:
computedGainFactors (ReferenceTFC_ID): | 0
powerOffsetPp_m: | 0
| :
ctfc2: | 1
| powerOffsetInformation:
| gainFactorInformation:
| signalledGainFactors:
| modeSpecificInfo:
| fdd:
gainFactorBetaC (GainFactor): | 11
gainFactorBetaD (GainFactor): | 15
referenceTFC_ID: | 0
powerOffsetPp_m: | 0
| prach_Partitioning:
| fdd:
| ASCSetting_FDD:
| accessServiceClass_FDD: Omit
| ASCSetting_FDD:
| accessServiceClass_FDD:
availableSignatureStartIndex: | 0
availableSignatureEndIndex: | 7
assignedSubChannelNumber: | 1111
| ASCSetting_FDD:
| accessServiceClass_FDD: Omit
| ASCSetting_FDD:
| accessServiceClass_FDD:
availableSignatureStartIndex: | 0
availableSignatureEndIndex: | 7
assignedSubChannelNumber: | 1111
| ASCSetting_FDD:
| accessServiceClass_FDD: Omit
| ASCSetting_FDD:
| accessServiceClass_FDD:
availableSignatureStartIndex: | 0
availableSignatureEndIndex: | 7
assignedSubChannelNumber: | 1111
| ASCSetting_FDD:
| accessServiceClass_FDD: Omit
| ASCSetting_FDD:
| accessServiceClass_FDD:
availableSignatureStartIndex: | 0
availableSignatureEndIndex: | 7
assignedSubChannelNumber: | 1111
| persistenceScalingFactorList:
PersistenceScalingFactor: | psf0_9
PersistenceScalingFactor: | psf0_9
PersistenceScalingFactor: | psf0_9
PersistenceScalingFactor: | psf0_9
PersistenceScalingFactor: | psf0_9
PersistenceScalingFactor: | psf0_9
| ac_To_ASC_MappingTable:
AC_To_ASC_Mapping: | 6
AC_To_ASC_Mapping: | 5
AC_To_ASC_Mapping: | 4
AC_To_ASC_Mapping: | 3
AC_To_ASC_Mapping: | 2
AC_To_ASC_Mapping: | 1
AC_To_ASC_Mapping: | 0
| modeSpecificInfo:
| fdd:
primaryCPICH_TX_Power: | 31
constantValue: | -10
| prach_PowerOffset:
powerRampStep: | 3
preambleRetransMax: | 4
| rach_TransmissionParameters:
mmax: | 2
nb01Min (NB01): | 3
nb01Max (NB01): | 10
| aich_Info:
channelisationCode256: | 3
sttd_Indicator: | false
aich_TransmissionTiming: | e0
| sCCPCH_SystemInformationList:
| SCCPCH_SystemInformation:
| secondaryCCPCH_Info:
| modeSpecificInfo:
| fdd:
dummy1 (PCPICH_UsageForChannelEst): | mayBeUsed
| dummy2: (SecondaryCPICH_Info) Omit
secondaryScramblingCode: | Omit
sttd_Indicator: | false
| sf_AndCodeNumber: (SF256_AndCodeNumber)
sf64: | 1
pilotSymbolExistence: | false
tfci_Existence: | true
positionFixedOrFlexible: | flexible
timingOffset: | 0
| tfcs:
| normalTFCI_Signalling: (ExplicitTFCS_Configuration)
| complete: (TFCS_ReconfAdd)
| ctfcSize:
| ctfc4Bit:
| :
ctfc4: | 0
| powerOffsetInformation: Omit
| :
ctfc4: | 1
| powerOffsetInformation: Omit
| :
ctfc4: | 2
| powerOffsetInformation: Omit
| :
ctfc4: | 3
| powerOffsetInformation: Omit
| :
ctfc4: | 4
| powerOffsetInformation: Omit
| :
ctfc4: | 5
| powerOffsetInformation: Omit
| :
ctfc4: | 6
| powerOffsetInformation: Omit
| :
ctfc4: | 8
| powerOffsetInformation: Omit
| fach_PCH_InformationList:
| FACH_PCH_Information:
| transportFormatSet:
| commonTransChTFS:
| tti:
| tti10: (CommonDynamicTF_InfoList)
| CommonDynamicTF_Info:
| rlc_Size:
| fdd:
| octetModeRLC_SizeInfoType2:
sizeType1: | 24
| numberOfTbSizeList:
| NumberOfTransportBlocks:
zero: |
| NumberOfTransportBlocks:
one: |
| logicalChannelList:
allSizes: |
| semistaticTF_Information:
| channelCodingType:
convolutional (CodingRate): | half
rateMatchingAttribute: | 230
crc_Size: | crc16
transportChannelIdentity: | 12
ctch_Indicator: | false
| FACH_PCH_Information:
| transportFormatSet:
| commonTransChTFS:
| tti:
| tti10: (CommonDynamicTF_InfoList)
| CommonDynamicTF_Info:
| rlc_Size:
| fdd:
| octetModeRLC_SizeInfoType2:
sizeType1: | 15
| numberOfTbSizeList:
| NumberOfTransportBlocks:
zero: |
| NumberOfTransportBlocks:
one: |
| NumberOfTransportBlocks:
small: | 2
| logicalChannelList:
allSizes: |
| semistaticTF_Information:
| channelCodingType:
convolutional (CodingRate): | half
rateMatchingAttribute: | 220
crc_Size: | crc16
transportChannelIdentity: | 13
ctch_Indicator: | false
| FACH_PCH_Information:
| transportFormatSet:
| commonTransChTFS:
| tti:
| tti10: (CommonDynamicTF_InfoList)
| CommonDynamicTF_Info:
| rlc_Size:
| fdd:
| octetModeRLC_SizeInfoType2:
sizeType2: | 3
| numberOfTbSizeList:
| NumberOfTransportBlocks:
zero: |
| NumberOfTransportBlocks:
one: |
| logicalChannelList:
allSizes: |
| semistaticTF_Information:
| channelCodingType:
turbo: |
rateMatchingAttribute: | 130
crc_Size: | crc16
transportChannelIdentity: | 14
ctch_Indicator: | false
| pich_Info:
| fdd:
channelisationCode256: | 2
pi_CountPerFrame: | e18
sttd_Indicator: | false
| cbs_DRX_Level1Information: Omit
| nonCriticalExtensions: Omit
| Outputs:
BITSTRING: |
[0] | 00 | 01 | 01 | 01 | 01 | 00 | 01 | 00
[8] | 00 | 11 | 11 | 10 | 00 | 00 | 00 | 00
[16] | 11 | 11 | 11 | 11 | 01 | 00 | 00 | 11
[24] | 11 | 11 | 11 | 11 | 11 | 11 | 11 | 01
[32] | 11 | 01 | 00 | 10 | 00 | 01 | 00 | 00
[40] | 11 | 11 | 00 | 00 | 00 | 10 | 10 | 01
[48] | 00 | 00 | 11 | 00 | 00 | 00 | 10 | 10
[56] | 10 | 10 | 01 | 01 | 01 | 01 | 10 | 00
[64] | 00 | 00 | 00 | 00 | 00 | 00 | 11 | 00
[72] | 11 | 00 | 01 | 01 | 10 | 11 | 01 | 01
[80] | 01 | 11 | 11 | 10 | 00 | 10 | 10 | 11
[88] | 10 | 10 | 00 | 00 | 11 | 11 | 11 | 10
[96] | 10 | 00 | 00 | 11 | 11 | 11 | 10 | 10
[104] | 00 | 00 | 11 | 11 | 11 | 10 | 10 | 00
[112] | 00 | 11 | 11 | 11 | 11 | 01 | 00 | 00
[120] | 00 | 00 | 00 | 00 | 00 | 00 | 00 | 11
[128] | 01 | 01 | 10 | 00 | 11 | 01 | 00 | 01
[136] | 00 | 00 | 11 | 11 | 11 | 01 | 00 | 11
[144] | 10 | 01 | 01 | 00 | 00 | 01 | 10 | 00
[152] | 01 | 00 | 00 | 11 | 00 | 10 | 10 | 00
[160] | 00 | 00 | 11 | 00 | 00 | 00 | 11 | 10
[168] | 00 | 00 | 01 | 00 | 00 | 00 | 01 | 01
[176] | 10 | 00 | 00 | 10 | 00 | 00 | 00 | 11
[184] | 10 | 00 | 00 | 00 | 00 | 10 | 00 | 10
[192] | 00 | 01 | 10 | 01 | 00 | 00 | 10 | 10
[200] | 01 | 10 | 01 | 00 | 00 | 10 | 10 | 00
[208] | 00 | 00 | 00 | 00 | 11 | 00 | 00 | 00
[216] | 01 | 00 | 01 | 00 | 01 | 01 | 11 | 00
[224] | 10 | 10 | 11 | 01 | 01 | 10 | 10 | 00
[232] | 00 | 00 | 00 | 00 | 01 | 11 | 10 | 00
[240] | 10 | 00 | 01 | 10 | 00 | 00 | 00 | 01
[248] | 01 | 10 | 11 | 01 | 10 | 11 | 01 | 10
[256] | 00 | 10 | 00 | 00 | 00 | 00 | 01 | 00
[264] | 00 | 11 | 00 | 00 | 10 | 00 | 10 | 01
[272] | 01 | 00 | 00 | 00 | 10 | 11 | 01 | 10
[280] | 10 | 00 | 00 | 00 | 01 | 00 | 00 |

#### MAC_DATA_REQ

RLC |  | MAC | @ 00:00:11.710

| Category: |  | Configuration
| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCCH
| CFN: |  | 156

| Message Details:
RLC PDU size (bits): | 176
RLC PDU (raw): |
[0] | 00 | 0E | 21 | 69 | C4 | 00 | 05 | 88
[8] | 28 | 02 | 11 | E0 | 14 | 00 | 00 | 0C
[16] | 74 | 04 | 26 | 00 | 00 | 20 |  |

#### MAC_DATA_REQ

RLC |  | MAC | @ 00:00:11.710

| Category: |  | Configuration
| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCCH
| CFN: |  | 156

| Message Details:
RLC PDU size (bits): | 176
RLC PDU (raw): |
[0] | 00 | 0E | 21 | 69 | C4 | 00 | 05 | 88
[8] | 28 | 02 | 11 | E0 | 14 | 00 | 00 | 0C
[16] | 74 | 04 | 26 | 00 | 00 | 20 |  |

#### PHY_DATA_REQ

MAC |  | PHY | @ 00:00:11.710

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCH
| CFN: |  | 156

| Message Details:
SIB repetition period: | 64
SIB position: | 20
SIB size: | 246
SIB (raw): |
[0] | 00 | 0E | 21 | 69 | C4 | 00 | 05 | 88
[8] | 28 | 02 | 11 | E0 | 14 | 00 | 00 | 0C
[16] | 74 | 04 | 26 | 00 | 00 | 20 | 00 | 00
[24] | 00 | 00 | 00 | 00 | 00 | 00 | 00 | 00
| SIB (decoded):
| TB 0:
MAC SDU (246 bits): |
[0] | 00 | 0E | 21 | 69 | C4 | 00 | 05 | 88
[8] | 28 | 02 | 11 | E0 | 14 | 00 | 00 | 0C
[16] | 74 | 04 | 26 | 00 | 00 | 20 | 00 | 00
[24] | 00 | 00 | 00 | 00 | 00 | 00 | 00 |

#### PHY_DATA_REQ

MAC |  | PHY | @ 00:00:11.730

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCH
| CFN: |  | 158

| Message Details:
SIB repetition period: | 64
SIB position: | 20
SIB size: | 246
SIB (raw): |
[0] | 00 | 0E | 21 | 69 | C4 | 00 | 05 | 88
[8] | 28 | 02 | 11 | E0 | 14 | 00 | 00 | 0C
[16] | 74 | 04 | 26 | 00 | 00 | 20 | 00 | 00
[24] | 00 | 00 | 00 | 00 | 00 | 00 | 00 | 00
| SIB (decoded):
| TB 0:
MAC SDU (246 bits): |
[0] | 00 | 0E | 21 | 69 | C4 | 00 | 05 | 88
[8] | 28 | 02 | 11 | E0 | 14 | 00 | 00 | 0C
[16] | 74 | 04 | 26 | 00 | 00 | 20 | 00 | 00
[24] | 00 | 00 | 00 | 00 | 00 | 00 | 00 |

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:11.740

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 22
bcch_ModificationTime: | Omit

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:11.750

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:11.750

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
noSegment: |

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA |  | RLC | @ 00:00:11.750

| Channel No: |  | 0 Name: BCCH

| Message Details:
| SIB repetition rate: 64
| SIB position: 44
| BCCH_BCH_Message:
| message:
| sfn_Prime: 0
| payload:
| noSegment: NULL
Layer 3 SDU: |
[0] | 00 | 00 |  |  |  |  |  |

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:11.750

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 18
bcch_ModificationTime: | Omit

#### MAC_DATA_REQ

RLC |  | MAC | @ 00:00:11.750

| Category: |  | Configuration
| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCCH
| CFN: |  | 160

| Message Details:
RLC PDU size (bits): | 184
RLC PDU (raw): |
[0] | 00 | 0E | 27 | 17 | 82 | 80 | 81 | 1B
[8] | 7A | 00 | 00 | 00 | 05 | B8 | C0 | 00
[16] | 80 | 12 | 10 | 23 | FF | FF | F8 |

#### MAC_DATA_REQ

RLC |  | MAC | @ 00:00:11.750

| Category: |  | Configuration
| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCCH
| CFN: |  | 160

| Message Details:
RLC PDU size (bits): | 168
RLC PDU (raw): |
[0] | 00 | 0E | 27 | 17 | 82 | 80 | 81 | 22
[8] | F0 | 00 | 00 | 00 | 0B | 71 | 80 | 01
[16] | 00 | 24 | 00 | 47 | 70 |  |  |

#### PHY_DATA_REQ

MAC |  | PHY | @ 00:00:11.750

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCH
| CFN: |  | 160

| Message Details:
SIB repetition period: | 64
SIB position: | 14
SIB size: | 246
SIB (raw): |
[0] | 00 | 0E | 27 | 17 | 82 | 80 | 81 | 1B
[8] | 7A | 00 | 00 | 00 | 05 | B8 | C0 | 00
[16] | 80 | 12 | 10 | 23 | FF | FF | F8 | 00
[24] | 00 | 00 | 00 | 00 | 00 | 00 | 00 | 00
| SIB (decoded):
| TB 0:
MAC SDU (246 bits): |
[0] | 00 | 0E | 27 | 17 | 82 | 80 | 81 | 1B
[8] | 7A | 00 | 00 | 00 | 05 | B8 | C0 | 00
[16] | 80 | 12 | 10 | 23 | FF | FF | F8 | 00
[24] | 00 | 00 | 00 | 00 | 00 | 00 | 00 |

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:11.770

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:11.770

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
| firstSegment:
sib_Type: | systemInformationBlockType5
seg_Count (SegCount): | 3
sib_Data_fixed: | 000101010100010000111110000000001111111101000011111111111111110111010010000100001111000000101001000011000000101010100101010110000000000000001100110001011011010101111110001010111010000011111110100000111111101000001111111010

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA |  | RLC | @ 00:00:11.770

| Channel No: |  | 0 Name: BCCH

| Message Details:
| SIB repetition rate: 64
| SIB position: 36
| BCCH_BCH_Message:
| message:
| sfn_Prime: 0
| payload:
| firstSegment:
| sib_Type: systemInformationBlockType5_SIB_Type [enum=5]
| seg_Count: 3
| sib_Data_fixed: 000101010100010000111110000000001111111101000011111111111111110111010010000100001111000000101001000011000000101010100101010110000000000000001100110001011011010101111110001010111010000011111110100000111111101000001111111010
Layer 3 SDU: |
[0] | 00 | 02 | 52 | 15 | 44 | 3E | 00 | FF
[8] | 43 | FF | FD | D2 | 10 | F0 | 29 | 0C
[16] | 0A | A5 | 58 | 00 | 0C | C5 | B5 | 7E
[24] | 2B | A0 | FE | 83 | FA | 0F | E8 |

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:11.770

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 19
bcch_ModificationTime: | Omit

#### PHY_DATA_REQ

MAC |  | PHY | @ 00:00:11.770

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCH
| CFN: |  | 162

| Message Details:
SIB repetition period: | 64
SIB position: | 62
SIB size: | 246
SIB (raw): |
[0] | 00 | 0E | 27 | 17 | 82 | 80 | 81 | 22
[8] | F0 | 00 | 00 | 00 | 0B | 71 | 80 | 01
[16] | 00 | 24 | 00 | 47 | 70 | FF | F8 | 00
[24] | 00 | 00 | 00 | 00 | 00 | 00 | 00 | 00
| SIB (decoded):
| TB 0:
MAC SDU (246 bits): |
[0] | 00 | 0E | 27 | 17 | 82 | 80 | 81 | 22
[8] | F0 | 00 | 00 | 00 | 0B | 71 | 80 | 01
[16] | 00 | 24 | 00 | 47 | 70 | FF | F8 | 00
[24] | 00 | 00 | 00 | 00 | 00 | 00 | 00 |

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:11.790

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:11.790

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
| subsequentSegment:
sib_Type: | systemInformationBlockType5
segmentIndex: | 1
sib_Data_fixed: | 000011111111010000000000000000001101011000110100010000111111010011100101000001100001000011001010000000110000001110000001000000010110000010000000111000000000100010000110010000101001100100001010000000000011000000010001000101

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA |  | RLC | @ 00:00:11.790

| Channel No: |  | 0 Name: BCCH

| Message Details:
| SIB repetition rate: 64
| SIB position: 38
| BCCH_BCH_Message:
| message:
| sfn_Prime: 0
| payload:
| subsequentSegment:
| sib_Type: systemInformationBlockType5_SIB_Type [enum=5]
| segmentIndex: 1
| sib_Data_fixed: 000011111111010000000000000000001101011000110100010000111111010011100101000001100001000011001010000000110000001110000001000000010110000010000000111000000000100010000110010000101001100100001010000000000011000000010001000101
Layer 3 SDU: |
[0] | 00 | 04 | 50 | 0F | F4 | 00 | 00 | D6
[8] | 34 | 43 | F4 | E5 | 06 | 10 | CA | 03
[16] | 03 | 81 | 01 | 60 | 80 | E0 | 08 | 86
[24] | 42 | 99 | 0A | 00 | 30 | 11 | 14 |

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:11.790

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 21
bcch_ModificationTime: | Omit

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:11.800

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:11.800

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
| lastSegmentShort:
sib_Type: | systemInformationBlockType5
segmentIndex: | 2
sib_Data_variable: | 1100101011010110100000000000011110001000011000000001011011011011011000100000000001000011000010001001010000001011011010000000010000

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA |  | RLC | @ 00:00:11.800

| Channel No: |  | 0 Name: BCCH

| Message Details:
| SIB repetition rate: 64
| SIB position: 42
| BCCH_BCH_Message:
| message:
| sfn_Prime: 0
| payload:
| lastSegmentShort:
| sib_Type: systemInformationBlockType5_SIB_Type [enum=5]
| segmentIndex: 2
| sib_Data_variable: 1100101011010110100000000000011110001000011000000001011011011011011000100000000001000011000010001001010000001011011010000000010000
Layer 3 SDU: |
[0] | 00 | 06 | 51 | 81 | CA | D6 | 80 | 07
[8] | 88 | 60 | 16 | DB | 62 | 00 | 43 | 08
[16] | 94 | 0B | 68 | 04 | 00 |  |  |

#### o_SIB_PER_Encoding

RRC |  | RRC | @ 00:00:11.800

| Category: |  | TSO

| Message Details:
| Inputs:
| SIB:
| sIB6: (SysInfoType6)
pich_PowerOffset: | -5
| modeSpecificInfo:
| fdd:
aich_PowerOffset: | -5
dummy (CSICH_PowerOffset): | Omit
| primaryCCPCH_Info: Omit
| prach_SystemInformationList: Omit
| sCCPCH_SystemInformationList: Omit
| cbs_DRX_Level1Information: Omit
| nonCriticalExtensions: Omit
| Outputs:
BITSTRING: |
[0] | 00 | 00 | 00 | 10 | 10 | 01 | 00 | 01

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:11.800

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 2
bcch_ModificationTime: | Omit

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:11.820

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:11.820

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
| completeSIB_List:
| CompleteSIBshort:
sib_Type: | systemInformationBlockType6
sib_Data_variable: | 0000001010010001

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA |  | RLC | @ 00:00:11.820

| Channel No: |  | 0 Name: BCCH

| Message Details:
| SIB repetition rate: 64
| SIB position: 4
| BCCH_BCH_Message:
| message:
| sfn_Prime: 0
| payload:
| completeSIB_List:
| CompleteSIB_List.element:
| sib_Type: systemInformationBlockType6_SIB_Type [enum=6]
| sib_Data_variable: 0000001010010001
Layer 3 SDU: |
[0] | 00 | 0E | 06 | 0F | 02 | 91 |  |

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:11.820

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 3
bcch_ModificationTime: | Omit

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:11.830

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:11.830

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
noSegment: |

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA |  | RLC | @ 00:00:11.830

| Channel No: |  | 0 Name: BCCH

| Message Details:
| SIB repetition rate: 64
| SIB position: 6
| BCCH_BCH_Message:
| message:
| sfn_Prime: 0
| payload:
| noSegment: NULL
Layer 3 SDU: |
[0] | 00 | 00 |  |  |  |  |  |

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:11.830

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 5
bcch_ModificationTime: | Omit

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:11.850

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:11.850

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
noSegment: |

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA |  | RLC | @ 00:00:11.850

| Channel No: |  | 0 Name: BCCH

| Message Details:
| SIB repetition rate: 64
| SIB position: 10
| BCCH_BCH_Message:
| message:
| sfn_Prime: 0
| payload:
| noSegment: NULL
Layer 3 SDU: |
[0] | 00 | 00 |  |  |  |  |  |

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:11.850

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 6
bcch_ModificationTime: | Omit

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:11.860

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:11.860

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
noSegment: |

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA |  | RLC | @ 00:00:11.860

| Channel No: |  | 0 Name: BCCH

| Message Details:
| SIB repetition rate: 64
| SIB position: 12
| BCCH_BCH_Message:
| message:
| sfn_Prime: 0
| payload:
| noSegment: NULL
Layer 3 SDU: |
[0] | 00 | 00 |  |  |  |  |  |

#### o_SIB_PER_Encoding

RRC |  | RRC | @ 00:00:11.860

| Category: |  | TSO

| Message Details:
| Inputs:
| SIB:
| sIB7: (SysInfoType7)
| modeSpecificInfo:
| fdd:
ul_Interference: | -100
| prach_Information_SIB5_List: (DynamicPersistenceLevelList)
DynamicPersistenceLevel: | 2
| prach_Information_SIB6_List: (DynamicPersistenceLevelList)
DynamicPersistenceLevel: | 2
expirationTimeFactor: | Omit
| nonCriticalExtensions: Omit
| Outputs:
BITSTRING: |
[0] | 10 | 00 | 00 | 10 | 10 | 00 | 00 | 00
[8] | 10 | 00 | 00 | 01 |  |  |  |

#### o_SIB_PER_Encoding

RRC |  | RRC | @ 00:00:11.860

| Category: |  | TSO

| Message Details:
| Inputs:
| SIB:
| sIB12: (SysInfoType12)
| fach_MeasurementOccasionInfo: Omit
| measurementControlSysInfo:
| use_of_HCS:
| hcs_not_used:
| cellSelectQualityMeasure:
| cpich_RSCP:
| intraFreqMeasurementSysInfo: (IntraFreqMeasurementSysInfo_RSCP) Omit
| interFreqMeasurementSysInfo: (InterFreqMeasurementSysInfo_RSCP) Omit
| interRATMeasurementSysInfo: (InterRATMeasurementSysInfo_B) Omit
| trafficVolumeMeasSysInfo: Omit
| dummy: (UE_InternalMeasurementSysInfo) Omit
| nonCriticalExtensions: Omit
| Outputs:
BITSTRING: |
[0] | 00 | 00 | 00 | 00 | 0 |  |  |

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:11.860

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 15
bcch_ModificationTime: | Omit

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:11.880

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:11.880

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
| completeSIB_List:
| CompleteSIBshort:
sib_Type: | systemInformationBlockType7
sib_Data_variable: | 100000101000000010000001

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA |  | RLC | @ 00:00:11.880

| Channel No: |  | 0 Name: BCCH

| Message Details:
| SIB repetition rate: 64
| SIB position: 30
| BCCH_BCH_Message:
| message:
| sfn_Prime: 0
| payload:
| completeSIB_List:
| CompleteSIB_List.element:
| sib_Type: systemInformationBlockType7_SIB_Type [enum=7]
| sib_Data_variable: 100000101000000010000001
Layer 3 SDU: |
[0] | 00 | 0E | 07 | 17 | 82 | 80 | 81 |

#### o_SIB_PER_Encoding

RRC |  | RRC | @ 00:00:11.880

| Category: |  | TSO

| Message Details:
| Inputs:
| SIB:
| sIB3: (SysInfoType3)
sib4indicator: | true
cellIdentity: | 0000000000000000000000000000
| cellSelectReselectInfo: (CellSelectReselectInfoSIB_3_4)
| mappingInfo: Omit
| cellSelectQualityMeasure:
cpich_RSCP: |
| modeSpecificInfo:
| fdd:
s_Intrasearch (S_SearchQual): | 8
s_Intersearch (S_SearchQual): | 8
s_SearchHCS (S_SearchRXLEV): | Omit
| rat_List: (RAT_FDD_InfoList)
| RAT_FDD_Info:
rat_Identifier: | gsm
s_SearchRAT (S_SearchQual): | -16
s_HCS_RAT (S_SearchRXLEV): | Omit
s_Limit_SearchRAT (S_SearchQual): | 0
q_QualMin: | -24
q_RxlevMin: | -40
q_Hyst_l_S (Q_Hyst_S): | 2
t_Reselection_S: | 0
| hcs_ServingCellInformation: Omit
maxAllowedUL_TX_Power: | 21
| cellAccessRestriction:
| cellBarred:
notBarred: |
cellReservedForOperatorUse (ReservedIndicator): | notReserved
cellReservationExtension (ReservedIndicator): | notReserved
| accessClassBarredList:
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
AccessClassBarred: | notBarred
| nonCriticalExtensions: Omit
| Outputs:
BITSTRING: |
[0] | 01 | 00 | 00 | 00 | 00 | 00 | 00 | 00
[8] | 00 | 00 | 00 | 00 | 00 | 00 | 00 | 00
[16] | 10 | 11 | 01 | 11 | 00 | 01 | 10 | 00
[24] | 00 | 00 | 00 | 00 | 00 | 01 | 00 | 00
[32] | 00 | 00 | 00 | 10 | 01 | 00 | 00 | 10
[40] | 00 | 00 | 01 | 00 | 01 | 11 | 11 | 11
[48] | 11 | 11 | 11 | 11 | 11 | 11 | 11 | 11

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:11.880

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 7
bcch_ModificationTime: | Omit

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:11.900

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:11.900

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
| completeSIB_List:
| CompleteSIBshort:
sib_Type: | systemInformationBlockType7
sib_Data_variable: | 100000101000000010000001
| CompleteSIBshort:
sib_Type: | systemInformationBlockType3
sib_Data_variable: | 0100000000000000000000000000000010110111000110000000000000010000000000100100001000000100011111111111111111111111

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA |  | RLC | @ 00:00:11.900

| Channel No: |  | 0 Name: BCCH

| Message Details:
| SIB repetition rate: 64
| SIB position: 14
| BCCH_BCH_Message:
| message:
| sfn_Prime: 0
| payload:
| completeSIB_List:
| CompleteSIB_List.element:
| sib_Type: systemInformationBlockType7_SIB_Type [enum=7]
| sib_Data_variable: 100000101000000010000001
| CompleteSIB_List.element:
| sib_Type: systemInformationBlockType3_SIB_Type [enum=3]
| sib_Data_variable: 0100000000000000000000000000000010110111000110000000000000010000000000100100001000000100011111111111111111111111
Layer 3 SDU: |
[0] | 00 | 0E | 27 | 17 | 82 | 80 | 81 | 1B
[8] | 7A | 00 | 00 | 00 | 05 | B8 | C0 | 00
[16] | 80 | 12 | 10 | 23 | FF | FF | F8 |

#### o_SIB_PER_Encoding

RRC |  | RRC | @ 00:00:11.900

| Category: |  | TSO

| Message Details:
| Inputs:
| SIB:
| sIB18: (SysInfoType18)
| idleModePLMNIdentities: (PLMNIdentitiesOfNeighbourCells)
| plmnsOfIntraFreqCellsList: Omit
| plmnsOfInterFreqCellsList: Omit
| plmnsOfInterRATCellsList: Omit
| connectedModePLMNIdentities: (PLMNIdentitiesOfNeighbourCells) Omit
| nonCriticalExtensions: Omit
| Outputs:
BITSTRING: |
[0] | 10 | 00 | 00 |  |  |  |  |

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:11.900

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 23
bcch_ModificationTime: | Omit

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:11.910

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:11.910

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
| completeSIB_List:
| CompleteSIBshort:
sib_Type: | systemInformationBlockType7
sib_Data_variable: | 100000101000000010000001
| CompleteSIBshort:
sib_Type: | systemInformationBlockType18
sib_Data_variable: | 100000

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA |  | RLC | @ 00:00:11.910

| Channel No: |  | 0 Name: BCCH

| Message Details:
| SIB repetition rate: 64
| SIB position: 46
| BCCH_BCH_Message:
| message:
| sfn_Prime: 0
| payload:
| completeSIB_List:
| CompleteSIB_List.element:
| sib_Type: systemInformationBlockType7_SIB_Type [enum=7]
| sib_Data_variable: 100000101000000010000001
| CompleteSIB_List.element:
| sib_Type: systemInformationBlockType18_SIB_Type [enum=26]
| sib_Data_variable: 100000
Layer 3 SDU: |
[0] | 00 | 0E | 27 | 17 | 82 | 80 | 81 | D0
[8] | 2C | 00 |  |  |  |  |  |

#### o_SIB_PER_Encoding

RRC |  | RRC | @ 00:00:11.910

| Category: |  | TSO

| Message Details:
| Inputs:
| SIB:
| sIB4: (SysInfoType4)
cellIdentity: | 0000000000000000000000000000
| cellSelectReselectInfo: (CellSelectReselectInfoSIB_3_4)
| mappingInfo: Omit
| cellSelectQualityMeasure:
cpich_RSCP: |
| modeSpecificInfo:
| fdd:
s_Intrasearch (S_SearchQual): | 8
s_Intersearch (S_SearchQual): | 8
s_SearchHCS (S_SearchRXLEV): | Omit
| rat_List: (RAT_FDD_InfoList)
| RAT_FDD_Info:
rat_Identifier: | gsm
s_SearchRAT (S_SearchQual): | -16
s_HCS_RAT (S_SearchRXLEV): | Omit
s_Limit_SearchRAT (S_SearchQual): | 0
q_QualMin: | -24
q_RxlevMin: | -40
q_Hyst_l_S (Q_Hyst_S): | 0
t_Reselection_S: | 0
| hcs_ServingCellInformation: Omit
maxAllowedUL_TX_Power: | 21
| cellAccessRestriction:
| cellBarred:
notBarred: |
cellReservedForOperatorUse (ReservedIndicator): | notReserved
cellReservationExtension (ReservedIndicator): | notReserved
| accessClassBarredList: Omit
| nonCriticalExtensions: Omit
| Outputs:
BITSTRING: |
[0] | 00 | 00 | 00 | 00 | 00 | 00 | 00 | 00
[8] | 00 | 00 | 00 | 00 | 00 | 00 | 00 | 01
[16] | 01 | 10 | 11 | 10 | 00 | 11 | 00 | 00
[24] | 00 | 00 | 00 | 00 | 00 | 10 | 00 | 00
[32] | 00 | 00 | 01 | 00 | 10 | 00 | 00 | 00
[40] | 00 | 00 | 10 | 00 | 11 | 10 | 11 | 1

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:11.910

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 31
bcch_ModificationTime: | Omit

#### MAC_DATA_REQ

RLC |  | MAC | @ 00:00:11.910

| Category: |  | Configuration
| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCCH
| CFN: |  | 176

| Message Details:
RLC PDU size (bits): | 16
RLC PDU (raw): |
[0] | 00 | 00 |  |  |  |  |  |

#### MAC_DATA_REQ

RLC |  | MAC | @ 00:00:11.910

| Category: |  | Configuration
| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCCH
| CFN: |  | 176

| Message Details:
RLC PDU size (bits): | 248
RLC PDU (raw): |
[0] | 00 | 02 | 52 | 15 | 44 | 3E | 00 | FF
[8] | 43 | FF | FD | D2 | 10 | F0 | 29 | 0C
[16] | 0A | A5 | 58 | 00 | 0C | C5 | B5 | 7E
[24] | 2B | A0 | FE | 83 | FA | 0F | E8 |

#### MAC_DATA_REQ

RLC |  | MAC | @ 00:00:11.910

| Category: |  | Configuration
| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCCH
| CFN: |  | 176

| Message Details:
RLC PDU size (bits): | 248
RLC PDU (raw): |
[0] | 00 | 04 | 50 | 0F | F4 | 00 | 00 | D6
[8] | 34 | 43 | F4 | E5 | 06 | 10 | CA | 03
[16] | 03 | 81 | 01 | 60 | 80 | E0 | 08 | 86
[24] | 42 | 99 | 0A | 00 | 30 | 11 | 14 |

#### MAC_DATA_REQ

RLC |  | MAC | @ 00:00:11.910

| Category: |  | Configuration
| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCCH
| CFN: |  | 176

| Message Details:
RLC PDU size (bits): | 168
RLC PDU (raw): |
[0] | 00 | 06 | 51 | 81 | CA | D6 | 80 | 07
[8] | 88 | 60 | 16 | DB | 62 | 00 | 43 | 08
[16] | 94 | 0B | 68 | 04 | 00 |  |  |

#### MAC_DATA_REQ

RLC |  | MAC | @ 00:00:11.910

| Category: |  | Configuration
| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCCH
| CFN: |  | 176

| Message Details:
RLC PDU size (bits): | 48
RLC PDU (raw): |
[0] | 00 | 0E | 06 | 0F | 02 | 91 |  |

#### MAC_DATA_REQ

RLC |  | MAC | @ 00:00:11.910

| Category: |  | Configuration
| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCCH
| CFN: |  | 176

| Message Details:
RLC PDU size (bits): | 16
RLC PDU (raw): |
[0] | 00 | 00 |  |  |  |  |  |

#### MAC_DATA_REQ

RLC |  | MAC | @ 00:00:11.910

| Category: |  | Configuration
| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCCH
| CFN: |  | 176

| Message Details:
RLC PDU size (bits): | 16
RLC PDU (raw): |
[0] | 00 | 00 |  |  |  |  |  |

#### MAC_DATA_REQ

RLC |  | MAC | @ 00:00:11.910

| Category: |  | Configuration
| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCCH
| CFN: |  | 176

| Message Details:
RLC PDU size (bits): | 16
RLC PDU (raw): |
[0] | 00 | 00 |  |  |  |  |  |

#### MAC_DATA_REQ

RLC |  | MAC | @ 00:00:11.910

| Category: |  | Configuration
| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCCH
| CFN: |  | 176

| Message Details:
RLC PDU size (bits): | 56
RLC PDU (raw): |
[0] | 00 | 0E | 07 | 17 | 82 | 80 | 81 |

#### PHY_DATA_REQ

MAC |  | PHY | @ 00:00:11.910

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCH
| CFN: |  | 176

| Message Details:
SIB repetition period: | 64
SIB position: | 44
SIB size: | 246
SIB (raw): |
[0] | 00 | 00 | 27 | 17 | 82 | 80 | 81 | 22
[8] | F0 | 00 | 00 | 00 | 0B | 71 | 80 | 01
[16] | 00 | 24 | 00 | 47 | 70 | FF | F8 | 00
[24] | 00 | 00 | 00 | 00 | 00 | 00 | 00 | 00
| SIB (decoded):
| TB 0:
MAC SDU (246 bits): |
[0] | 00 | 00 | 27 | 17 | 82 | 80 | 81 | 22
[8] | F0 | 00 | 00 | 00 | 0B | 71 | 80 | 01
[16] | 00 | 24 | 00 | 47 | 70 | FF | F8 | 00
[24] | 00 | 00 | 00 | 00 | 00 | 00 | 00 |

#### MAC_DATA_REQ

RLC |  | MAC | @ 00:00:11.920

| Category: |  | Configuration
| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCCH
| CFN: |  | 177

| Message Details:
RLC PDU size (bits): | 184
RLC PDU (raw): |
[0] | 00 | 0E | 27 | 17 | 82 | 80 | 81 | 1B
[8] | 7A | 00 | 00 | 00 | 05 | B8 | C0 | 00
[16] | 80 | 12 | 10 | 23 | FF | FF | F8 |

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:11.930

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:11.930

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
| completeSIB_List:
| CompleteSIBshort:
sib_Type: | systemInformationBlockType7
sib_Data_variable: | 100000101000000010000001
| CompleteSIBshort:
sib_Type: | systemInformationBlockType4
sib_Data_variable: | 00000000000000000000000000000001011011100011000000000000001000000000010010000000000010001110111

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA |  | RLC | @ 00:00:11.930

| Channel No: |  | 0 Name: BCCH

| Message Details:
| SIB repetition rate: 64
| SIB position: 62
| BCCH_BCH_Message:
| message:
| sfn_Prime: 0
| payload:
| completeSIB_List:
| CompleteSIB_List.element:
| sib_Type: systemInformationBlockType7_SIB_Type [enum=7]
| sib_Data_variable: 100000101000000010000001
| CompleteSIB_List.element:
| sib_Type: systemInformationBlockType4_SIB_Type [enum=4]
| sib_Data_variable: 00000000000000000000000000000001011011100011000000000000001000000000010010000000000010001110111
Layer 3 SDU: |
[0] | 00 | 0E | 27 | 17 | 82 | 80 | 81 | 22
[8] | F0 | 00 | 00 | 00 | 0B | 71 | 80 | 01
[16] | 00 | 24 | 00 | 47 | 70 |  |  |

#### o_SIB_PER_Encoding

RRC |  | RRC | @ 00:00:11.930

| Category: |  | TSO

| Message Details:
| Inputs:
| SIB:
| sIB11: (SysInfoType11)
sib12indicator: | true
| fach_MeasurementOccasionInfo: Omit
| measurementControlSysInfo:
| use_of_HCS:
| hcs_not_used:
| cellSelectQualityMeasure:
| cpich_RSCP:
| intraFreqMeasurementSysInfo: (IntraFreqMeasurementSysInfo_RSCP)
intraFreqMeasurementID (MeasurementIdentity):
| Omit
| intraFreqCellInfoSI_List: (IntraFreqCellInfoSI_List_RSCP)
| removedIntraFreqCellList: Omit
| newIntraFreqCellList: (NewIntraFreqCellSI_List_RSCP)
| NewIntraFreqCellSI_RSCP:
intraFreqCellID:
| 0
| cellInfo: (CellInfoSI_RSCP)
cellIndividualOffset:
| Omit
| referenceTimeDifferenceToCell: Omit
| modeSpecificInfo:
| fdd:
| primaryCPICH_Info:
primaryScramblingCode:
| 100
primaryCPICH_TX_Power: | Omit
readSFN_Indicator: | false
tx_DiversityIndicator: | false
| cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP) Omit
| NewIntraFreqCellSI_RSCP:
intraFreqCellID: | 1
| cellInfo: (CellInfoSI_RSCP)
cellIndividualOffset: | Omit
| referenceTimeDifferenceToCell: Omit
| modeSpecificInfo:
| fdd:
| primaryCPICH_Info:
primaryScramblingCode: | 150
primaryCPICH_TX_Power: | Omit
readSFN_Indicator: | true
tx_DiversityIndicator: | false
| cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP) Omit
| NewIntraFreqCellSI_RSCP:
intraFreqCellID: | 2
| cellInfo: (CellInfoSI_RSCP)
cellIndividualOffset: | Omit
| referenceTimeDifferenceToCell: Omit
| modeSpecificInfo:
| fdd:
| primaryCPICH_Info:
primaryScramblingCode: | 200
primaryCPICH_TX_Power: | Omit
readSFN_Indicator: | true
tx_DiversityIndicator: | false
| cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP) Omit
| NewIntraFreqCellSI_RSCP:
intraFreqCellID: | 6
| cellInfo: (CellInfoSI_RSCP)
cellIndividualOffset: | Omit
| referenceTimeDifferenceToCell: Omit
| modeSpecificInfo:
| fdd:
| primaryCPICH_Info:
primaryScramblingCode: | 400
primaryCPICH_TX_Power: | Omit
readSFN_Indicator: | true
tx_DiversityIndicator: | false
| cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP) Omit
| NewIntraFreqCellSI_RSCP:
intraFreqCellID: | 7
| cellInfo: (CellInfoSI_RSCP)
cellIndividualOffset: | Omit
| referenceTimeDifferenceToCell: Omit
| modeSpecificInfo:
| fdd:
| primaryCPICH_Info:
primaryScramblingCode: | 450
primaryCPICH_TX_Power: | Omit
readSFN_Indicator: | true
tx_DiversityIndicator: | false
| cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP) Omit
| intraFreqMeasQuantity:
filterCoefficient: | Omit
| modeSpecificInfo:
| fdd:
intraFreqMeasQuantity_FDD: | cpich_RSCP
| intraFreqReportingQuantityForRACH: Omit
maxReportedCellsOnRACH: | Omit
| reportingInfoForCellDCH:
| intraFreqReportingQuantity:
| activeSetReportingQuantities: (CellReportingQuantities)
dummy (SFN_SFN_OTD_Type): | noReport
cellIdentity_reportingIndicator: | true
cellSynchronisationInfoReportingIndicator: | false
| modeSpecificInfo:
| fdd:
cpich_Ec_N0_reportingIndicator: | false
cpich_RSCP_reportingIndicator: | true
pathloss_reportingIndicator: | false
| monitoredSetReportingQuantities: (CellReportingQuantities)
dummy (SFN_SFN_OTD_Type): | noReport
cellIdentity_reportingIndicator: | true
cellSynchronisationInfoReportingIndicator: | true
| modeSpecificInfo:
| fdd:
cpich_Ec_N0_reportingIndicator: | false
cpich_RSCP_reportingIndicator: | true
pathloss_reportingIndicator: | false
| detectedSetReportingQuantities: (CellReportingQuantities) Omit
| measurementReportingMode:
measurementReportTransferMode (TransferMode): | acknowledgedModeRLC
periodicalOrEventTrigger: | eventTrigger
| reportCriteria: (CellDCH_ReportCriteria)
| intraFreqReportingCriteria:
| eventCriteriaList: (IntraFreqEventCriteriaList)
| IntraFreqEventCriteria:
| event: (IntraFreqEvent)
| e1a: (Event1a)
triggeringCondition (TriggeringCondition2): | monitoredSetCellsOnly
reportingRange: | 5
| forbiddenAffectCellList: Omit
w: | 1
reportDeactivationThreshold: | t2
reportingAmount: | ra4
reportingInterval: | ri4
hysteresis: | 0
timeToTrigger: | ttt640
| reportingCellStatus:
withinActiveAndOrMonitoredUsedFreq (MaxNumberOfReportingCellsType1): | e3
| IntraFreqEventCriteria:
| event: (IntraFreqEvent)
| e1b: (Event1b)
triggeringCondition (TriggeringCondition1): | activeSetCellsOnly
reportingRange: | 5
| forbiddenAffectCellList: Omit
w: | 1
hysteresis: | 0
timeToTrigger: | ttt640
| reportingCellStatus:
withinActiveAndOrMonitoredUsedFreq (MaxNumberOfReportingCellsType1): | e3
| IntraFreqEventCriteria:
| event: (IntraFreqEvent)
| e1c: (Event1c)
replacementActivationThreshold: | t3
reportingAmount: | ra4
reportingInterval: | ri4
hysteresis: | 0
timeToTrigger: | ttt640
| reportingCellStatus:
withinActiveAndOrMonitoredUsedFreq (MaxNumberOfReportingCellsType1): | e3

| interFreqMeasurementSysInfo: (InterFreqMeasurementSysInfo_RSCP)
| interFreqCellInfoSI_List: (InterFreqCellInfoSI_List_RSCP)
| removedInterFreqCellList: Omit
| newInterFreqCellList: (NewInterFreqCellSI_List_RSCP)
| NewInterFreqCellSI_RSCP:
interFreqCellID: | 3
| frequencyInfo:
| modeSpecificInfo:
| fdd: (FrequencyInfoFDD)
uarfcn_UL (UARFCN): | Omit
uarfcn_DL (UARFCN): | 10837
| cellInfo: (CellInfoSI_RSCP)
cellIndividualOffset: | Omit
| referenceTimeDifferenceToCell: Omit
| modeSpecificInfo:
| fdd:
| primaryCPICH_Info:
primaryScramblingCode: | 250
primaryCPICH_TX_Power: | Omit
readSFN_Indicator: | false
tx_DiversityIndicator: | false
| cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP) Omit
| NewInterFreqCellSI_RSCP:
interFreqCellID: | 4
| frequencyInfo: Omit
| cellInfo: (CellInfoSI_RSCP)
cellIndividualOffset: | Omit
| referenceTimeDifferenceToCell: Omit
| modeSpecificInfo:
| fdd:
| primaryCPICH_Info:
primaryScramblingCode: | 300
primaryCPICH_TX_Power: | Omit
readSFN_Indicator: | false
tx_DiversityIndicator: | false
| cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP) Omit
| NewInterFreqCellSI_RSCP:
interFreqCellID: | 5
| frequencyInfo: Omit
| cellInfo: (CellInfoSI_RSCP)
cellIndividualOffset: | Omit
| referenceTimeDifferenceToCell: Omit
| modeSpecificInfo:
| fdd:
| primaryCPICH_Info:
primaryScramblingCode: | 350
primaryCPICH_TX_Power: | Omit
readSFN_Indicator: | false
tx_DiversityIndicator: | false
| cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP) Omit

| interRATMeasurementSysInfo: (InterRATMeasurementSysInfo_B) Omit

| trafficVolumeMeasSysInfo: Omit

| dummy: (UE_InternalMeasurementSysInfo) Omit

| nonCriticalExtensions: Omit

| Outputs:
BITSTRING: |
[0] | 00 | 10 | 00 | 00 | 11 | 01 | 10 | 01
[8] | 00 | 01 | 00 | 10 | 00 | 00 | 00 | 00
[16] | 10 | 00 | 11 | 00 | 10 | 00 | 01 | 00
[24] | 00 | 10 | 00 | 01 | 00 | 10 | 01 | 01
[32] | 10 | 10 | 10 | 00 | 10 | 00 | 00 | 10
[40] | 01 | 10 | 01 | 00 | 01 | 01 | 00 | 11
[48] | 00 | 00 | 01 | 01 | 10 | 01 | 00 | 00
[56] | 10 | 10 | 01 | 11 | 00 | 00 | 10 | 11
[64] | 10 | 00 | 01 | 01 | 00 | 00 | 10 | 00
[72] | 10 | 00 | 10 | 00 | 11 | 00 | 10 | 01
[80] | 01 | 01 | 01 | 00 | 00 | 00 | 01 | 00
[88] | 10 | 10 | 00 | 01 | 01 | 00 | 10 | 10
[96] | 10 | 00 | 01 | 10 | 00 | 01 | 00 | 10
[104] | 10 | 00 | 10 | 00 | 00 | 10 | 10 | 00
[112] | 01 | 00 | 00 | 11 | 00 | 00 | 10 | 01
[120] | 01 | 00 | 10 | 01 | 10 | 10 | 10 | 10
[128] | 00 | 01 | 10 | 00 | 01 | 00 | 10 | 10
[136] | 10 | 00 | 10 | 11 | 00 | 01 | 10 | 01
[144] | 01 | 01 | 00 | 10 | 10 | 10 | 10 | 00
[152] | 01 | 00 | 11 | 11 | 10 | 10 | 00 | 10
[160] | 00 | 10 | 00 | 00 | 01 | 01 | 00 | 10
[168] | 11 | 00 | 00 | 10 | 00 | 10 | 10 | 00
[176] | 01 | 01 | 01 | 01 | 11 | 10 | 00 |

#### PHY_DATA_REQ

MAC |  | PHY | @ 00:00:11.930

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCH
| CFN: |  | 178

| Message Details:
SIB repetition period: | 64
SIB position: | 36
SIB size: | 246
SIB (raw): |
[0] | 00 | 02 | 52 | 15 | 44 | 3E | 00 | FF
[8] | 43 | FF | FD | D2 | 10 | F0 | 29 | 0C
[16] | 0A | A5 | 58 | 00 | 0C | C5 | B5 | 7E
[24] | 2B | A0 | FE | 83 | FA | 0F | E8 | 00
| SIB (decoded):
| TB 0:
MAC SDU (246 bits): |
[0] | 00 | 02 | 52 | 15 | 44 | 3E | 00 | FF
[8] | 43 | FF | FD | D2 | 10 | F0 | 29 | 0C
[16] | 0A | A5 | 58 | 00 | 0C | C5 | B5 | 7E
[24] | 2B | A0 | FE | 83 | FA | 0F | E8 |

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:11.940

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 30
bcch_ModificationTime: | Omit

#### PHY_DATA_REQ

MAC |  | PHY | @ 00:00:11.950

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCH
| CFN: |  | 180

| Message Details:
SIB repetition period: | 64
SIB position: | 38
SIB size: | 246
SIB (raw): |
[0] | 00 | 04 | 50 | 0F | F4 | 00 | 00 | D6
[8] | 34 | 43 | F4 | E5 | 06 | 10 | CA | 03
[16] | 03 | 81 | 01 | 60 | 80 | E0 | 08 | 86
[24] | 42 | 99 | 0A | 00 | 30 | 11 | 14 | 00
| SIB (decoded):
| TB 0:
MAC SDU (246 bits): |
[0] | 00 | 04 | 50 | 0F | F4 | 00 | 00 | D6
[8] | 34 | 43 | F4 | E5 | 06 | 10 | CA | 03
[16] | 03 | 81 | 01 | 60 | 80 | E0 | 08 | 86
[24] | 42 | 99 | 0A | 00 | 30 | 11 | 14 |

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:11.960

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:11.960

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
noSegment: |

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA |  | RLC | @ 00:00:11.960

| Channel No: |  | 0 Name: BCCH

| Message Details:
| SIB repetition rate: 64
| SIB position: 60
| BCCH_BCH_Message:
| message:
| sfn_Prime: 0
| payload:
| noSegment: NULL
Layer 3 SDU: |
[0] | 00 | 00 |  |  |  |  |  |

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:11.960

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 29
bcch_ModificationTime: | Omit

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:11.970

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:11.970

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
noSegment:

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA |  | RLC | @ 00:00:11.970

| Channel No: |  | 0 Name: BCCH

| Message Details:
| SIB repetition rate: 64
| SIB position: 58
| BCCH_BCH_Message:
| message:
| sfn_Prime: 0
| payload:
| noSegment: NULL
Layer 3 SDU: |
[0] | 00 | 00 |  |  |  |  |  |

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:11.970

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 26
bcch_ModificationTime: | Omit

#### PHY_DATA_REQ

MAC |  | PHY | @ 00:00:11.970

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCH
| CFN: |  | 182

| Message Details:
SIB repetition period: | 64
SIB position: | 42
SIB size: | 246
SIB (raw): |
[0] | 00 | 06 | 51 | 81 | CA | D6 | 80 | 07
[8] | 88 | 60 | 16 | DB | 62 | 00 | 43 | 08
[16] | 94 | 0B | 68 | 04 | 00 | E0 | 08 | 86
[24] | 42 | 99 | 0A | 00 | 30 | 11 | 14 | 00
| SIB (decoded):
| TB 0:
MAC SDU (246 bits): |
[0] | 00 | 06 | 51 | 81 | CA | D6 | 80 | 07
[8] | 88 | 60 | 16 | DB | 62 | 00 | 43 | 08
[16] | 94 | 0B | 68 | 04 | 00 | E0 | 08 | 86
[24] | 42 | 99 | 0A | 00 | 30 | 11 | 14 |

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:11.990

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:11.990

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
| firstSegment:
sib_Type: | systemInformationBlockType11
seg_Count (SegCount): | 2
sib_Data_fixed: | 001000001101100100010010000000001000110010000100001000010010010110101000100000100110010001010011000001011001000010100111000010111000010100001000100010001100100101010100000001001010000101001010100001100001001010001000001010

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA |  | RLC | @ 00:00:11.990

| Channel No: |  | 0 Name: BCCH

| Message Details:
| SIB repetition rate: 64
| SIB position: 52
| BCCH_BCH_Message:
| message:
| sfn_Prime: 0
| payload:
| firstSegment:
| sib_Type: systemInformationBlockType11_SIB_Type [enum=11]
| seg_Count: 2
| sib_Data_fixed: 001000001101100100010010000000001000110010000100001000010010010110101000100000100110010001010011000001011001000010100111000010111000010100001000100010001100100101010100000001001010000101001010100001100001001010001000001010

Layer 3 SDU: |
[0] | 00 | 02 | B1 | 20 | D9 | 12 | 00 | 8C
[8] | 84 | 21 | 25 | A8 | 82 | 64 | 53 | 05
[16] | 90 | A7 | 0B | 85 | 08 | 88 | C9 | 54
[24] | 04 | A1 | 4A | 86 | 12 | 88 | 28 |

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:11.990

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 27
bcch_ModificationTime: | Omit

#### PHY_DATA_REQ

MAC |  | PHY | @ 00:00:11.990

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCH
| CFN: |  | 184

| Message Details:
SIB repetition period: | 64
SIB position: | 4
SIB size: | 246
SIB (raw): |
[0] | 00 | 0E | 06 | 0F | 02 | 91 | 80 | 07
[8] | 88 | 60 | 16 | DB | 62 | 00 | 43 | 08
[16] | 94 | 0B | 68 | 04 | 00 | E0 | 08 | 86
[24] | 42 | 99 | 0A | 00 | 30 | 11 | 14 | 00
| SIB (decoded):
| TB 0:
MAC SDU (246 bits): |
[0] | 00 | 0E | 06 | 0F | 02 | 91 | 80 | 07
[8] | 88 | 60 | 16 | DB | 62 | 00 | 43 | 08
[16] | 94 | 0B | 68 | 04 | 00 | E0 | 08 | 86
[24] | 42 | 99 | 0A | 00 | 30 | 11 | 14 |

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:12.000

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId: | 0
| routingInfo:
rB_Identity:
| -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:12.000

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1
| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0
| payload:
| lastSegmentShort:
sib_Type: | systemInformationBlockType11
segmentIndex: | 1
sib_Data_variable: | 000100001100001001010010011010101000011000010010101000101100011001010100101010100001001111101000100010000001010010110000100010100001010101111000

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA |  | RLC | @ 00:00:12.000

| Channel No: |  | 0 Name: BCCH

| Message Details:
| SIB repetition rate: 64
| SIB position: 54
| BCCH_BCH_Message:
| message:
| sfn_Prime: 0
| payload:
| lastSegmentShort:
| sib_Type: systemInformationBlockType11_SIB_Type [enum=11]
| segmentIndex: 1
| sib_Data_variable: 000100001100001001010010011010101000011000010010101000101100011001010100101010100001001111101000100010000001010010110000100010100001010101111000

Layer 3 SDU: |
[0] | 00 | 06 | B0 | 8F | 10 | C2 | 52 | 6A
[8] | 86 | 12 | A2 | C6 | 54 | AA | 13 | E8
[16] | 88 | 14 | B0 | 8A | 15 | 78 |  |

#### o_SIB_PER_Encoding

RRC |  | RRC | @ 00:00:12.000

| Category: |  | TSO

| Message Details:
| Inputs:
| SIB:
| sIB12: (SysInfoType12)
| fach_MeasurementOccasionInfo: Omit
| measurementControlSysInfo:
| use_of_HCS:
| hcs_not_used:
| cellSelectQualityMeasure:
| cpich_RSCP:
| intraFreqMeasurementSysInfo: (IntraFreqMeasurementSysInfo_RSCP) Omit
| interFreqMeasurementSysInfo: (InterFreqMeasurementSysInfo_RSCP) Omit

| interRATMeasurementSysInfo: (InterRATMeasurementSysInfo_B) Omit

| trafficVolumeMeasSysInfo: Omit

| dummy: (UE_InternalMeasurementSysInfo) Omit

| nonCriticalExtensions: Omit

| Outputs:
BITSTRING: |
[0] | 00 | 00 | 00 | 00 | 0 |  |  |

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:12.000

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0
| routingInfo:
rB_Identity: | -1

ratType: | fdd
| configMessage: (CmacSysinfoConfigReq)
sg_REP:
| 6
sg_POS: | 11
bcch_ModificationTime: | Omit

#### PHY_DATA_REQ

MAC |  | PHY | @ 00:00:12.010

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCH
| CFN: |  | 186

| Message Details:
SIB repetition period: | 64
SIB position: | 6
SIB size: | 246
SIB (raw): |
[0] | 00 | 00 | 06 | 0F | 02 | 91 | 80 | 07
[8] | 88 | 60 | 16 | DB | 62 | 00 | 43 | 08
[16] | 94 | 0B | 68 | 04 | 00 | E0 | 08 | 86
[24] | 42 | 99 | 0A | 00 | 30 | 11 | 14 | 00

| SIB (decoded):
| TB 0:
MAC SDU (246 bits): |
[0] | 00 | 00 | 06 | 0F | 02 | 91 | 80 | 07
[8] | 88 | 60 | 16 | DB | 62 | 00 | 43 | 08
[16] | 94 | 0B | 68 | 04 | 00 | E0 | 08 | 86
[24] | 42 | 99 | 0A | 00 | 30 | 11 | 14 |

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:12.020

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_CNF:
cellId:
| 0

| routingInfo:
rB_Identity:
| -1

#### RLC_TR_DATA_REQ

RRC |  | LLA | @ 00:00:12.020

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| RLC_TR_DATA_REQ:
cellId: | 0

| routingInfo:
rB_Identity: | -1

| tM_message:
| bCCH_BCH_Message:
| message: (SystemInformation_BCH)
sfn_Prime: | 0

| payload:
| completeSIB_List:
| CompleteSIBshort:
sib_Type: | systemInformationBlockType12
sib_Data_variable: | 000000000

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA |  | RLC | @ 00:00:12.020

| Channel No: |  | 0 Name: BCCH

| Message Details:
| SIB repetition rate: 64

| SIB position: 22

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

completeSIB_List:

CompleteSIB_List.element:

sib_Type: systemInformationBlockType12_SIB_Type [enum=12]

sib_Data_variable: 000000000

Layer 3 SDU:

[0]

00 0E 0C 08 00 00

#### CMAC_SYSINFO_Config_REQ

RRC |  | LLA | @ 00:00:12.020

| Channel ID: |  | RbBcch
| Cell ID: |  | 0

| Message Details:
| CMAC_SYSINFO_Config_REQ:
cellId: | 0

| routingInfo:
rB_Identity: | -1

ratType:

fdd

| configMessage: (CmacSysinfoConfigReq)
sg_REP: | 6
sg_POS: | 13
bcch_ModificationTime: | Omit

#### PHY_DATA_REQ

MAC |  | PHY | @ 00:00:12.030

| BTS unit: |  | 1:1
| Channel No: |  | 0 Name: BCH
| CFN: |  | 188

| Message Details: | SIB repetition period: | 64 SIB position: | 10 SIB size: | 246 SIB (raw): | [0] | 00 | 00 | 06 | 0F | 02 | 91 | 80 | 07 [8] | 88 | 60 | 16 | DB | 62 | 00 | 43 | 08 [16] | 94 | 0B | 68 | 04 | 00 | E0 | 08 | 86 [24] | 42 | 99 | 0A | 00 | 30 | 11 | 14 | 00

| SIB (decoded):
| TB 0:
MAC SDU (246 bits): |
[0] | 00 | 00 | 06 | 0F | 02 | 91 | 80 | 07
[8] | 88 | 60 | 16 | DB | 62 | 00 | 43 | 08
[16] | 94 | 0B | 68 | 04 | 00 | E0 | 08 | 86
[24] | 42 | 99 | 0A | 00 | 30 | 11 | 14 |

#### CMAC_SYSINFO_Config_CNF

LLA |  | RRC | @ 00:00:12.040

| Channel ID: |  | RbBcch | Cell ID: |  | 0

| Message Details: |  | CMAC_SYSINFO_Config_CNF: | cellId: | 0

| routingInfo: | rB_Identity: | -1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:00:12.040

Channel ID: RbBcch
Cell ID: 0

Message Details:

RLC_TR_DATA_REQ:

cellId:0

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

noSegment:

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:00:12.040

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 26

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

noSegment: NULL

Layer 3 SDU:

[0]00 00

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:00:12.040

Channel ID: RbBcch
Cell ID: 0

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:0

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:14
bcch_ModificationTime: Omit

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:00:12.050

Channel ID: RbBcch
Cell ID: 0

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:0

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:00:12.050

Channel ID: RbBcch
Cell ID: 0

Message Details:

RLC_TR_DATA_REQ:

cellId:0

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

noSegment:

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:00:12.050

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 28

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

noSegment: NULL

Layer 3 SDU:

[0]00 00

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:00:12.050

Channel ID: RbBcch
Cell ID: 0

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:0

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:15
bcch_ModificationTime: Omit

#### PHY_DATA_REQ

MAC PHY @ 00:00:12.050

BTS unit: 1:1
Channel No: 0 Name: BCH
CFN: 190

Message Details:

SIB repetition period:64
SIB position:12
SIB size:246
SIB (raw):

[0]00 00 06 0F 02 91 80 07
[8]88 60 16 DB 62 00 43 08
[16]94 0B 68 04 00 E0 08 86
[24]42 99 0A 00 30 11 14 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 00 06 0F 02 91 80 07
[8]88 60 16 DB 62 00 43 08
[16]94 0B 68 04 00 E0 08 86
[24]42 99 0A 00 30 11 14

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:00:12.070

Channel ID: RbBcch
Cell ID: 0

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:0

routingInfo:

rB_Identity:-1

#### o_SIB_PER_Encoding

RRC RRC @ 00:00:12.070

Category: TSO

Message Details:

Inputs:

SIB:

sIB7: (SysInfoType7)

modeSpecificInfo:

fdd:

ul_Interference:-100

prach_Information_SIB5_List: (DynamicPersistenceLevelList)

DynamicPersistenceLevel:2

prach_Information_SIB6_List: (DynamicPersistenceLevelList)

DynamicPersistenceLevel:2

expirationTimeFactor: Omit

nonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]10 00 00 10 10 00 00 00
[8]10 00 00 01

#### RLC_TR_DATA_REQ

RRC LLA @ 00:00:12.070

Channel ID: RbBcch
Cell ID: 0

Message Details:

RLC_TR_DATA_REQ:

cellId:0

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

completeSIB_List:

CompleteSIBshort:

sib_Type:systemInformationBlockType7
sib_Data_variable:100000101000000010000001

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:00:12.070

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 30

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

completeSIB_List:

CompleteSIB_List.element:

sib_Type: systemInformationBlockType7_SIB_Type [enum=7]

sib_Data_variable: 100000101000000010000001

Layer 3 SDU:

[0]00 0E 07 17 82 80 81

#### o_SIB_PER_Encoding

RRC RRC @ 00:00:12.070

Category: TSO

Message Details:

Inputs:

SIB:

sIB18: (SysInfoType18)

idleModePLMNIdentities: (PLMNIdentitiesOfNeighbourCells)

plmnsOfIntraFreqCellsList: Omit

plmnsOfInterFreqCellsList: Omit

plmnsOfInterRATCellsList: Omit

connectedModePLMNIdentities: (PLMNIdentitiesOfNeighbourCells) Omit

nonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]10 00 00

#### o_SIB_PER_Encoding

RRC RRC @ 00:00:12.070

Category: TSO

Message Details:

Inputs:

SIB:

sIB7: (SysInfoType7)

modeSpecificInfo:

fdd:

ul_Interference:-100

prach_Information_SIB5_List: (DynamicPersistenceLevelList)

DynamicPersistenceLevel:2

prach_Information_SIB6_List: (DynamicPersistenceLevelList)

DynamicPersistenceLevel:2

expirationTimeFactor: Omit

nonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]10 00 00 10 10 00 00 00
[8]10 00 00 01

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:00:12.070

Channel ID: RbBcch
Cell ID: 0

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:0

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:23
bcch_ModificationTime: Omit

#### MAC_DATA_REQ

RLC MAC @ 00:00:12.070

Category: Configuration
BTS unit: 1:1
Channel No: 0 Name: BCCH
CFN: 192

Message Details:

RLC PDU size (bits):80
RLC PDU (raw):

[0]00 0E 27 17 82 80 81 D0
[8]2C 00

#### MAC_DATA_REQ

RLC MAC @ 00:00:12.070

Category: Configuration
BTS unit: 1:1
Channel No: 0 Name: BCCH
CFN: 192

Message Details:

RLC PDU size (bits):168
RLC PDU (raw):

[0]00 0E 27 17 82 80 81 22
[8]F0 00 00 00 0B 71 80 01
[16]00 24 00 47 70

#### MAC_DATA_REQ

RLC MAC @ 00:00:12.070

Category: Configuration
BTS unit: 1:1
Channel No: 0 Name: BCCH
CFN: 192

Message Details:

RLC PDU size (bits):16
RLC PDU (raw):

[0]00 00

#### MAC_DATA_REQ

RLC MAC @ 00:00:12.070

Category: Configuration
BTS unit: 1:1
Channel No: 0 Name: BCCH
CFN: 192

Message Details:

RLC PDU size (bits):16
RLC PDU (raw):

[0]00 00

#### MAC_DATA_REQ

RLC MAC @ 00:00:12.070

Category: Configuration
BTS unit: 1:1
Channel No: 0 Name: BCCH
CFN: 192

Message Details:

RLC PDU size (bits):248
RLC PDU (raw):

[0]00 02 B1 20 D9 12 00 8C
[8]84 21 25 A8 82 64 53 05
[16]90 A7 0B 85 08 88 C9 54
[24]04 A1 4A 86 12 88 28

#### MAC_DATA_REQ

RLC MAC @ 00:00:12.070

Category: Configuration
BTS unit: 1:1
Channel No: 0 Name: BCCH
CFN: 192

Message Details:

RLC PDU size (bits):176
RLC PDU (raw):

[0]00 06 B0 8F 10 C2 52 6A
[8]86 12 A2 C6 54 AA 13 E8
[16]88 14 B0 8A 15 78

#### MAC_DATA_REQ

RLC MAC @ 00:00:12.070

Category: Configuration
BTS unit: 1:1
Channel No: 0 Name: BCCH
CFN: 192

Message Details:

RLC PDU size (bits):48
RLC PDU (raw):

[0]00 0E 0C 08 00 00

#### MAC_DATA_REQ

RLC MAC @ 00:00:12.070

Category: Configuration
BTS unit: 1:1
Channel No: 0 Name: BCCH
CFN: 192

Message Details:

RLC PDU size (bits):16
RLC PDU (raw):

[0]00 00

#### PHY_DATA_REQ

MAC PHY @ 00:00:12.070

BTS unit: 1:1
Channel No: 0 Name: BCH
CFN: 192

Message Details:

SIB repetition period:64
SIB position:30
SIB size:246
SIB (raw):

[0]00 0E 07 17 82 80 81 07
[8]88 60 16 DB 62 00 43 08
[16]94 0B 68 04 00 E0 08 86
[24]42 99 0A 00 30 11 14 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 0E 07 17 82 80 81 07
[8]88 60 16 DB 62 00 43 08
[16]94 0B 68 04 00 E0 08 86
[24]42 99 0A 00 30 11 14

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:00:12.080

Channel ID: RbBcch
Cell ID: 0

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:0

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:00:12.080

Channel ID: RbBcch
Cell ID: 0

Message Details:

RLC_TR_DATA_REQ:

cellId:0

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

completeSIB_List:

CompleteSIBshort:

sib_Type:systemInformationBlockType7
sib_Data_variable:100000101000000010000001

CompleteSIBshort:

sib_Type:systemInformationBlockType18
sib_Data_variable:100000

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:00:12.080

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 46

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

completeSIB_List:

CompleteSIB_List.element:

sib_Type: systemInformationBlockType7_SIB_Type [enum=7]

sib_Data_variable: 100000101000000010000001

CompleteSIB_List.element:

sib_Type: systemInformationBlockType18_SIB_Type [enum=26]

sib_Data_variable: 100000

Layer 3 SDU:

[0]00 0E 27 17 82 80 81 D0
[8]2C 00

#### o_SIB_PER_Encoding

RRC RRC @ 00:00:12.080

Category: TSO

Message Details:

Inputs:

SIB:

sB1: (SysInfoTypeSB1)

sib_ReferenceList:

SchedulingInformationSIB:

sib_Type: (SIB_TypeAndTag)

sysInfoType6 (CellValueTag):2

scheduling: (SchedulingInformation)

scheduling:

segCount: Omit

sib_Pos:

rep64:2

sib_PosOffsetInfo: (SibOFF_List) Omit

SchedulingInformationSIB:

sib_Type: (SIB_TypeAndTag)

sysInfoType7:

scheduling: (SchedulingInformation)

scheduling:

segCount: Omit

sib_Pos:

rep16:7

sib_PosOffsetInfo: (SibOFF_List) Omit

SchedulingInformationSIB:

sib_Type: (SIB_TypeAndTag)

sysInfoType11 (CellValueTag):2

scheduling: (SchedulingInformation)

scheduling:

segCount:2

sib_Pos:

rep64:26

sib_PosOffsetInfo: (SibOFF_List)

SibOFF:so2

SchedulingInformationSIB:

sib_Type: (SIB_TypeAndTag)

sysInfoType12 (CellValueTag):2

scheduling: (SchedulingInformation)

scheduling:

segCount: Omit

sib_Pos:

rep64:11

sib_PosOffsetInfo: (SibOFF_List) Omit

SchedulingInformationSIB:

sib_Type: (SIB_TypeAndTag)

sysInfoType18 (CellValueTag):2

scheduling: (SchedulingInformation)

scheduling:

segCount: Omit

sib_Pos:

rep64:23

sib_PosOffsetInfo: (SibOFF_List) Omit

nonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]00 01 00 00 10 10 10 00
[8]10 00 00 10 00 11 00 00
[16]01 01 11 01 01 00 11 10
[24]00 10 10 01 10 10 00 00
[32]00 00 01 01 10 10 00 10
[40]00 10 11 11 00 10 10 00
[48]10 01 01 11

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:00:12.080

Channel ID: RbBcch
Cell ID: 0

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:0

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:4
sg_POS:1
bcch_ModificationTime: Omit

#### PHY_DATA_REQ

MAC PHY @ 00:00:12.090

BTS unit: 1:1
Channel No: 0 Name: BCH
CFN: 194

Message Details:

SIB repetition period:64
SIB position:14
SIB size:246
SIB (raw):

[0]00 0E 27 17 82 80 81 1B
[8]7A 00 00 00 05 B8 C0 00
[16]80 12 10 23 FF FF F8 86
[24]42 99 0A 00 30 11 14 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 0E 27 17 82 80 81 1B
[8]7A 00 00 00 05 B8 C0 00
[16]80 12 10 23 FF FF F8 86
[24]42 99 0A 00 30 11 14

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:00:12.100

Channel ID: RbBcch
Cell ID: 0

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:0

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:00:12.100

Channel ID: RbBcch
Cell ID: 0

Message Details:

RLC_TR_DATA_REQ:

cellId:0

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

completeSIB_List:

CompleteSIBshort:

sib_Type:schedulingBlock1
sib_Data_variable:00010000101010001000001000110000010111010100111000101001101000000000010110100010001011110010100010010111

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:00:12.100

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 16

SIB position: 2

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

completeSIB_List:

CompleteSIB_List.element:

sib_Type: schedulingBlock1_SIB_Type [enum=27]

sib_Data_variable: 00010000101010001000001000110000010111010100111000101001101000000000010110100010001011110010100010010111

Layer 3 SDU:

[0]00 0E 1B 67 10 A8 82 30
[8]5D 4E 29 A0 05 A2 2F 28
[16]97

#### o_SIB_PER_Encoding

RRC RRC @ 00:00:12.100

Category: TSO

Message Details:

Inputs:

SIB:

mIB: (MasterInformationBlock)

mib_ValueTag:1

plmn_Type:

gsm_MAP:

plmn_Identity:

mcc:

Digit:0
Digit:0
Digit:1

mnc:

Digit:0
Digit:1

sibSb_ReferenceList:

SchedulingInformationSIBSb:

sibSb_Type: (SIBSb_TypeAndTag)

sysInfoTypeSB1 (CellValueTag):2

scheduling: (SchedulingInformation)

scheduling:

segCount: Omit

sib_Pos:

rep16:1

sib_PosOffsetInfo: (SibOFF_List) Omit

SchedulingInformationSIBSb:

sibSb_Type: (SIBSb_TypeAndTag)

sysInfoType1 (PLMN_ValueTag):2

scheduling: (SchedulingInformation)

scheduling:

segCount: Omit

sib_Pos:

rep64:10

sib_PosOffsetInfo: (SibOFF_List) Omit

SchedulingInformationSIBSb:

sibSb_Type: (SIBSb_TypeAndTag)

sysInfoType2 (CellValueTag):2

scheduling: (SchedulingInformation)

scheduling:

segCount: Omit

sib_Pos:

rep64:10

sib_PosOffsetInfo: (SibOFF_List) Omit

SchedulingInformationSIBSb:

sibSb_Type: (SIBSb_TypeAndTag)

sysInfoType3 (CellValueTag):2

scheduling: (SchedulingInformation)

scheduling:

segCount: Omit

sib_Pos:

rep64:7

sib_PosOffsetInfo: (SibOFF_List) Omit

SchedulingInformationSIBSb:

sibSb_Type: (SIBSb_TypeAndTag)

sysInfoType4 (CellValueTag):2

scheduling: (SchedulingInformation)

scheduling:

segCount: Omit

sib_Pos:

rep64:31

sib_PosOffsetInfo: (SibOFF_List) Omit

SchedulingInformationSIBSb:

sibSb_Type: (SIBSb_TypeAndTag)

sysInfoType5 (CellValueTag):2

scheduling: (SchedulingInformation)

scheduling:

segCount:3

sib_Pos:

rep64:18

sib_PosOffsetInfo: (SibOFF_List)

SibOFF:so2
SibOFF:so4

nonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]00 00 00 00 00 00 00 00
[8]01 00 00 00 00 10 01 01
[16]10 10 10 10 00 01 00 01
[24]00 00 00 00 00 00 10 00
[32]10 00 10 10 00 00 10 10
[40]00 10 00 10 10 00 01 00
[48]10 00 10 00 01 11 00 01
[56]10 10 00 10 01 11 11 00
[64]10 00 11 10 01 00 10 01
[72]00 10 00 01 00 00 00 01

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:00:12.100

Channel ID: RbBcch
Cell ID: 0

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:0

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:3
sg_POS:0
bcch_ModificationTime: Omit

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:00:12.110

Channel ID: RbBcch
Cell ID: 0

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:0

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:00:12.110

Channel ID: RbBcch
Cell ID: 0

Message Details:

RLC_TR_DATA_REQ:

cellId:0

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

completeSIB_List:

CompleteSIBshort:

sib_Type:masterInformationBlock
sib_Data_variable:0000000000000000010000000010010110101010000100010000000000001000100010100000101000100010100001001000100001110001101000100111110010001110010010010010000100000001

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:00:12.110

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 8

SIB position: 0

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

completeSIB_List:

CompleteSIB_List.element:

sib_Type: masterInformationBlock_SIB_Type [enum=0]

sib_Data_variable: 0000000000000000010000000010010110101010000100010000000000001000100010100000101000100010100001001000100001110001101000100111110010001110010010010010000100000001

Layer 3 SDU:

[0]00 0E 00 9F 00 00 40 25
[8]AA 11 00 08 8A 0A 22 84
[16]88 71 A2 7C 8E 49 21 01

#### PHY_DATA_REQ

MAC PHY @ 00:00:12.110

BTS unit: 1:1
Channel No: 0 Name: BCH
CFN: 196

Message Details:

SIB repetition period:64
SIB position:46
SIB size:246
SIB (raw):

[0]00 0E 27 17 82 80 81 D0
[8]2C 00 00 00 05 B8 C0 00
[16]80 12 10 23 FF FF F8 86
[24]42 99 0A 00 30 11 14 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 0E 27 17 82 80 81 D0
[8]2C 00 00 00 05 B8 C0 00
[16]80 12 10 23 FF FF F8 86
[24]42 99 0A 00 30 11 14

#### CPHY_Cell_Config_REQ

RRC LLA @ 00:00:12.130

Cell ID: 3

Message Details:

CPHY_Cell_Config_REQ:

cellId:3
tcell:321
sfnOffset:3000

frequencyInfo:

modeSpecificInfo:

fdd: (FrequencyInfoFDD)

uarfcn_UL (UARFCN): Omit
uarfcn_DL (UARFCN):10837

primaryScramblingCode_SS:250

cellTxPowerLevel:

defaultCellTxPowerLvl:

dLTxAttenuationLevel:30

#### MAC_DATA_REQ

RLC MAC @ 00:00:12.130

Category: Configuration
BTS unit: 1:1
Channel No: 0 Name: BCCH
CFN: 198

Message Details:

RLC PDU size (bits):16
RLC PDU (raw):

[0]00 00

#### MAC_DATA_REQ

RLC MAC @ 00:00:12.130

Category: Configuration
BTS unit: 1:1
Channel No: 0 Name: BCCH
CFN: 198

Message Details:

RLC PDU size (bits):56
RLC PDU (raw):

[0]00 0E 07 17 82 80 81

#### MAC_DATA_REQ

RLC MAC @ 00:00:12.130

Category: Configuration
BTS unit: 1:1
Channel No: 0 Name: BCCH
CFN: 198

Message Details:

RLC PDU size (bits):80
RLC PDU (raw):

[0]00 0E 27 17 82 80 81 D0
[8]2C 00

#### MAC_DATA_REQ

RLC MAC @ 00:00:12.130

Category: Configuration
BTS unit: 1:1
Channel No: 0 Name: BCCH
CFN: 198

Message Details:

RLC PDU size (bits):136
RLC PDU (raw):

[0]00 0E 1B 67 10 A8 82 30
[8]5D 4E 29 A0 05 A2 2F 28
[16]97

#### MAC_DATA_REQ

RLC MAC @ 00:00:12.130

Category: Configuration
BTS unit: 1:1
Channel No: 0 Name: BCCH
CFN: 198

Message Details:

RLC PDU size (bits):192
RLC PDU (raw):

[0]00 0E 00 9F 00 00 40 25
[8]AA 11 00 08 8A 0A 22 84
[16]88 71 A2 7C 8E 49 21 01

#### PHY_DATA_REQ

MAC PHY @ 00:00:12.130

BTS unit: 1:1
Channel No: 0 Name: BCH
CFN: 198

Message Details:

SIB repetition period:64
SIB position:62
SIB size:246
SIB (raw):

[0]00 0E 27 17 82 80 81 22
[8]F0 00 00 00 0B 71 80 01
[16]00 24 00 47 70 FF F8 86
[24]42 99 0A 00 30 11 14 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 0E 27 17 82 80 81 22
[8]F0 00 00 00 0B 71 80 01
[16]00 24 00 47 70 FF F8 86
[24]42 99 0A 00 30 11 14

#### PHY_DATA_REQ

MAC PHY @ 00:00:12.150

BTS unit: 1:1
Channel No: 0 Name: BCH
CFN: 200

Message Details:

SIB repetition period:64
SIB position:60
SIB size:246
SIB (raw):

[0]00 00 27 17 82 80 81 22
[8]F0 00 00 00 0B 71 80 01
[16]00 24 00 47 70 FF F8 86
[24]42 99 0A 00 30 11 14 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 00 27 17 82 80 81 22
[8]F0 00 00 00 0B 71 80 01
[16]00 24 00 47 70 FF F8 86
[24]42 99 0A 00 30 11 14

#### PHY_DATA_REQ

MAC PHY @ 00:00:12.170

BTS unit: 1:1
Channel No: 0 Name: BCH
CFN: 202

Message Details:

SIB repetition period:64
SIB position:58
SIB size:246
SIB (raw):

[0]00 00 27 17 82 80 81 22
[8]F0 00 00 00 0B 71 80 01
[16]00 24 00 47 70 FF F8 86
[24]42 99 0A 00 30 11 14 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 00 27 17 82 80 81 22
[8]F0 00 00 00 0B 71 80 01
[16]00 24 00 47 70 FF F8 86
[24]42 99 0A 00 30 11 14

#### PHY_DATA_REQ

MAC PHY @ 00:00:12.190

BTS unit: 1:1
Channel No: 0 Name: BCH
CFN: 204

Message Details:

SIB repetition period:64
SIB position:52
SIB size:246
SIB (raw):

[0]00 02 B1 20 D9 12 00 8C
[8]84 21 25 A8 82 64 53 05
[16]90 A7 0B 85 08 88 C9 54
[24]04 A1 4A 86 12 88 28 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 02 B1 20 D9 12 00 8C
[8]84 21 25 A8 82 64 53 05
[16]90 A7 0B 85 08 88 C9 54
[24]04 A1 4A 86 12 88 28

#### PHY_DATA_REQ

MAC PHY @ 00:00:12.210

BTS unit: 1:1
Channel No: 0 Name: BCH
CFN: 206

Message Details:

SIB repetition period:64
SIB position:54
SIB size:246
SIB (raw):

[0]00 06 B0 8F 10 C2 52 6A
[8]86 12 A2 C6 54 AA 13 E8
[16]88 14 B0 8A 15 78 C9 54
[24]04 A1 4A 86 12 88 28 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 06 B0 8F 10 C2 52 6A
[8]86 12 A2 C6 54 AA 13 E8
[16]88 14 B0 8A 15 78 C9 54
[24]04 A1 4A 86 12 88 28

#### CPHY BTS Frequency REQ

LLA PHY @ 00:00:12.230

BTS unit: 1:2
CFN: 208

Message Details:

Configuration Parameters:

Down Link Frequency:2167400000
Up Link Frequency:1977400000

#### PHY_DATA_REQ

MAC PHY @ 00:00:12.230

BTS unit: 1:1
Channel No: 0 Name: BCH
CFN: 208

Message Details:

SIB repetition period:64
SIB position:22
SIB size:246
SIB (raw):

[0]00 0E 0C 08 00 00 52 6A
[8]86 12 A2 C6 54 AA 13 E8
[16]88 14 B0 8A 15 78 C9 54
[24]04 A1 4A 86 12 88 28 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 0E 0C 08 00 00 52 6A
[8]86 12 A2 C6 54 AA 13 E8
[16]88 14 B0 8A 15 78 C9 54
[24]04 A1 4A 86 12 88 28

#### CPHY BTS Frequency CNF

PHY LLA @ 00:00:12.230

BTS unit: 1:2
CFN: 208

Message Details:

#### PHY_DATA_REQ

MAC PHY @ 00:00:12.250

BTS unit: 1:1
Channel No: 0 Name: BCH
CFN: 210

Message Details:

SIB repetition period:64
SIB position:26
SIB size:246
SIB (raw):

[0]00 00 0C 08 00 00 52 6A
[8]86 12 A2 C6 54 AA 13 E8
[16]88 14 B0 8A 15 78 C9 54
[24]04 A1 4A 86 12 88 28 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 00 0C 08 00 00 52 6A
[8]86 12 A2 C6 54 AA 13 E8
[16]88 14 B0 8A 15 78 C9 54
[24]04 A1 4A 86 12 88 28

#### CPHY_Cell_Config_CNF

LLA RRC @ 00:00:12.270

Cell ID: 3

Message Details:

CPHY_Cell_Config_CNF:

cellId:3

#### CPHY_RL_Setup_REQ

RRC LLA @ 00:00:12.270

Channel ID: P-CPICH
Cell ID: 3

Message Details:

CPHY_RL_Setup_REQ:

cellId:3

routingInfo:

physicalChannelIdentity:0

ratType:fdd

setupMessage: (CphyRlSetupReq)

physicalChannelInfo:

primaryCPICHInfo:

dl_TxPower_PCPICH:-55
txdiversityIndicator:false

#### PHY_DATA_REQ

MAC PHY @ 00:00:12.270

BTS unit: 1:1
Channel No: 0 Name: BCH
CFN: 212

Message Details:

SIB repetition period:64
SIB position:28
SIB size:246
SIB (raw):

[0]00 00 0C 08 00 00 52 6A
[8]86 12 A2 C6 54 AA 13 E8
[16]88 14 B0 8A 15 78 C9 54
[24]04 A1 4A 86 12 88 28 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 00 0C 08 00 00 52 6A
[8]86 12 A2 C6 54 AA 13 E8
[16]88 14 B0 8A 15 78 C9 54
[24]04 A1 4A 86 12 88 28

#### PHY_DATA_REQ

MAC PHY @ 00:00:12.290

BTS unit: 1:1
Channel No: 0 Name: BCH
CFN: 214

Message Details:

SIB repetition period:64
SIB position:30
SIB size:246
SIB (raw):

[0]00 0E 07 17 82 80 81 6A
[8]86 12 A2 C6 54 AA 13 E8
[16]88 14 B0 8A 15 78 C9 54
[24]04 A1 4A 86 12 88 28 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 0E 07 17 82 80 81 6A
[8]86 12 A2 C6 54 AA 13 E8
[16]88 14 B0 8A 15 78 C9 54
[24]04 A1 4A 86 12 88 28

#### PHY_DATA_REQ

MAC PHY @ 00:00:12.310

BTS unit: 1:1
Channel No: 0 Name: BCH
CFN: 216

Message Details:

SIB repetition period:64
SIB position:46
SIB size:246
SIB (raw):

[0]00 0E 27 17 82 80 81 D0
[8]2C 00 A2 C6 54 AA 13 E8
[16]88 14 B0 8A 15 78 C9 54
[24]04 A1 4A 86 12 88 28 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 0E 27 17 82 80 81 D0
[8]2C 00 A2 C6 54 AA 13 E8
[16]88 14 B0 8A 15 78 C9 54
[24]04 A1 4A 86 12 88 28

#### PHY_DATA_REQ

MAC PHY @ 00:00:12.330

BTS unit: 1:1
Channel No: 0 Name: BCH
CFN: 218

Message Details:

SIB repetition period:16
SIB position:2
SIB size:246
SIB (raw):

[0]00 0E 1B 67 10 A8 82 30
[8]5D 4E 29 A0 05 A2 2F 28
[16]97 14 B0 8A 15 78 C9 54
[24]04 A1 4A 86 12 88 28 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 0E 1B 67 10 A8 82 30
[8]5D 4E 29 A0 05 A2 2F 28
[16]97 14 B0 8A 15 78 C9 54
[24]04 A1 4A 86 12 88 28

#### PHY_DATA_REQ

MAC PHY @ 00:00:12.350

BTS unit: 1:1
Channel No: 0 Name: BCH
CFN: 220

Message Details:

SIB repetition period:8
SIB position:0
SIB size:246
SIB (raw):

[0]00 0E 00 9F 00 00 40 25
[8]AA 11 00 08 8A 0A 22 84
[16]88 71 A2 7C 8E 49 21 01
[24]04 A1 4A 86 12 88 28 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 0E 00 9F 00 00 40 25
[8]AA 11 00 08 8A 0A 22 84
[16]88 71 A2 7C 8E 49 21 01
[24]04 A1 4A 86 12 88 28

#### CPHY Radio Link Setup REQ

LLA PHY @ 00:00:12.360

BTS unit: 1:2
Channel No: 0 Name: P_CPICH
CFN: 221

Message Details:

Configuration Parameters:

Channel Offset:7680
Scrambling Code:4000
Symbol Rate:15k
Channelization Code:0
Adjust Time:0
Power in dBm:-65
Tx Diversity:Off
NumOfDpdch:0

#### CPHY Radio Link Setup CNF

PHY LLA @ 00:00:12.360

BTS unit: 1:2
Channel No: 0 Name: P_CPICH
CFN: 221

Message Details:

#### CPHY_RL_Setup_CNF

LLA RRC @ 00:00:12.380

Channel ID: P-CPICH
Cell ID: 3

Message Details:

CPHY_RL_Setup_CNF:

cellId:3

routingInfo:

physicalChannelIdentity:0

#### CPHY_RL_Setup_REQ

RRC LLA @ 00:00:12.380

Channel ID: P-SCH
Cell ID: 3

Message Details:

CPHY_RL_Setup_REQ:

cellId:3

routingInfo:

physicalChannelIdentity:1

ratType:fdd

setupMessage: (CphyRlSetupReq)

physicalChannelInfo:

primarySCHInfo:

tstdIndicator:false
dl_TxPower:-5

#### CPHY Radio Link Setup REQ

LLA PHY @ 00:00:12.550

BTS unit: 1:2
Channel No: 0 Name: P_SCH
CFN: 240

Message Details:

Configuration Parameters:

Channel Offset:7680
Adjust Time:0
Power in dBm:-70
Tx Diversity:Off
NumOfDpdch:0

#### CPHY Radio Link Setup CNF

PHY LLA @ 00:00:12.550

BTS unit: 1:2
Channel No: 0 Name: P_SCH
CFN: 240

Message Details:

#### CPHY_RL_Setup_CNF

LLA RRC @ 00:00:12.580

Channel ID: P-SCH
Cell ID: 3

Message Details:

CPHY_RL_Setup_CNF:

cellId:3

routingInfo:

physicalChannelIdentity:1

#### CPHY_RL_Setup_REQ

RRC LLA @ 00:00:12.580

Channel ID: S-SCH
Cell ID: 3

Message Details:

CPHY_RL_Setup_REQ:

cellId:3

routingInfo:

physicalChannelIdentity:2

ratType:fdd

setupMessage: (CphyRlSetupReq)

physicalChannelInfo:

secondarySCHInfo:

tstdIndicator:false
dl_TxPower:-5

#### CPHY Radio Link Setup REQ

LLA PHY @ 00:00:12.710

BTS unit: 1:2
Channel No: 0 Name: S_SCH
CFN: 0

Message Details:

Configuration Parameters:

Channel Offset:7680
Adjust Time:0
Power in dBm:-70
Tx Diversity:Off
NumOfDpdch:0

#### CPHY Radio Link Setup CNF

PHY LLA @ 00:00:12.710

BTS unit: 1:2
Channel No: 0 Name: S_SCH
CFN: 0

Message Details:

#### CPHY_RL_Setup_CNF

LLA RRC @ 00:00:12.720

Channel ID: S-SCH
Cell ID: 3

Message Details:

CPHY_RL_Setup_CNF:

cellId:3

routingInfo:

physicalChannelIdentity:2

#### CPHY_RL_Setup_REQ

RRC LLA @ 00:00:12.720

Channel ID: P-CCPCH
Cell ID: 3

Message Details:

CPHY_RL_Setup_REQ:

cellId:3

routingInfo:

physicalChannelIdentity:4

ratType:fdd

setupMessage: (CphyRlSetupReq)

physicalChannelInfo:

primaryCCPCHInfo:

sttd_Indicator:false
dl_TxPower:-2

#### CPHY Radio Link Setup REQ

LLA PHY @ 00:00:12.780

BTS unit: 1:2
Channel No: 0 Name: P_CCPCH
CFN: 7

Message Details:

Configuration Parameters:

Channel Offset:7680
SFN Offset:0
Scrambling Code:4000
Symbol Rate:15k
Channelization Code:1
Adjust Time:0
Power in dBm:-67
Tx Diversity:Off
NumOfDpdch:1

#### CPHY Radio Link Setup CNF

PHY LLA @ 00:00:12.780

BTS unit: 1:2
Channel No: 0 Name: P_CCPCH
CFN: 7

Message Details:

#### CPHY_RL_Setup_CNF

LLA RRC @ 00:00:12.800

Channel ID: P-CCPCH
Cell ID: 3

Message Details:

CPHY_RL_Setup_CNF:

cellId:3

routingInfo:

physicalChannelIdentity:4

#### CPHY_TrCH_Config_REQ

RRC LLA @ 00:00:12.800

Channel ID: P-CCPCH
Cell ID: 3

Message Details:

CPHY_TrCH_Config_REQ:

cellId:3

routingInfo:

physicalChannelIdentity:4

ratType:fdd

trchConfigType:

nonDch:

configMessage: (CphyTrchConfigReq)

activationTime: (SS_ActivationTime)

activateNow:

ulconnectedTrCHList: Omit

ulTFCS: (TFCS) Omit

dlconnectedTrCHList:

:

trchid (TransportChannelIdentity):11
dl_TransportChannelType (SS_DL_TransportChannelType):bch

transportChannelInfo: (CommonOrDedicatedTFS)

tti:

tti20: (CommonOrDedicatedTF_InfoList)

CommonOrDedicatedTF_Info:

tb_Size:246

numberOfTbSizeList:

NumberOfTransportBlocks:

one:

logicalChannelList:

configured:

semistaticTF_Information:

channelCodingType:

convolutional (CodingRate):half

rateMatchingAttribute:1
crc_Size:crc16

dlTFCS: (TFCS)

normalTFCI_Signalling: (ExplicitTFCS_Configuration)

complete: (TFCS_ReconfAdd)

ctfcSize:

ctfc2Bit:

:

ctfc2:0

powerOffsetInformation:

gainFactorInformation:

signalledGainFactors:

modeSpecificInfo:

fdd:

gainFactorBetaC (GainFactor):11

gainFactorBetaD (GainFactor):15
referenceTFC_ID:0

powerOffsetPp_m: Omit

#### CPHY Transport Channel Configuration REQ

LLA PHY @ 00:00:12.820

BTS unit: 1:2
Channel No: 0 Name: P_CCPCH
CFN: 11

Message Details:

Configuration Parameters:

DTX Position:Flexible
Second Interleave:On
Puncture Limit:0
CCTrCH Length:270
Number Of Transport Channels:1

Transport Channels:

Item Number 0:

Transport Channel Parameters:

Transport Channel:

Name:BCH
Identity:0

TTI (ms):20
EP Type:1/2 Rate Convolutional Coding
CRC Size:16
RM Attribute:1
First Interleave:On
Number Of Transport Formats:2

Transport Format Set:

Transport Format 0:

Number Of Transport Blocks:0
Transport Block Size In Bits:0

Transport Format 1:

Number Of Transport Blocks:1
Transport Block Size In Bits:246

RM Maximum Length:540

Transport Format Combination Set:

Number Of Transport Format Combinations:2

Transport Format Combinations 0:

Transport Format:0

Transport Format Combinations 1:

Transport Format:1

#### CPHY Transport Channel Configuration CNF

PHY LLA @ 00:00:12.820

BTS unit: 1:2
Channel No: 0 Name: P_CCPCH
CFN: 11

Message Details:

#### CPHY_TrCH_Config_CNF

LLA RRC @ 00:00:12.830

Channel ID: P-CCPCH
Cell ID: 3

Message Details:

CPHY_TrCH_Config_CNF:

cellId:3

routingInfo:

physicalChannelIdentity:4

#### CMAC_Config_REQ

RRC LLA @ 00:00:12.830

Channel ID: P-CCPCH
Cell ID: 3

Message Details:

CMAC_Config_REQ:

cellId:3

routingInfo:

physicalChannelIdentity:4

ratType:fdd

configMessage:

setup: (CmacConfigReq)

activationTime: (SS_ActivationTime)

activateNow:

uE_Info:

u_RNTI: Omit

c_RNTI: Omit

trCHInfo:

ulconnectedTrCHList: Omit

ulTFCS: (TFCS) Omit

dlconnectedTrCHList:

:

trchid (TransportChannelIdentity):11

transportChannelInfo: (CommonOrDedicatedTFS)

tti:

tti20: (CommonOrDedicatedTF_InfoList)

CommonOrDedicatedTF_Info:

tb_Size:246

numberOfTbSizeList:

NumberOfTransportBlocks:

one:

logicalChannelList:

configured:

semistaticTF_Information:

channelCodingType:

convolutional (CodingRate):half

rateMatchingAttribute:1
crc_Size:crc16

dlTFCS: (TFCS)

normalTFCI_Signalling: (ExplicitTFCS_Configuration)

complete: (TFCS_ReconfAdd)

ctfcSize:

ctfc2Bit:

:

ctfc2:0

powerOffsetInformation:

gainFactorInformation:

signalledGainFactors:

modeSpecificInfo:

fdd:

gainFactorBetaC (GainFactor):11

gainFactorBetaD (GainFactor):15
referenceTFC_ID:0

powerOffsetPp_m: Omit

trCH_LogCHMapping: (TrCH_LogCHMappingList1)

ulconnectedTrCHList: Omit

dlconnectedTrCHList:

:

trchid (TransportChannelIdentity):11

trCH_LogCHMappingList:

TrCH_LogicalChannelMapping:

logicalChannel_Mapping:

dl_LogicalChannelMapping: (SS_DL_LogicalChannelMapping)

macHeaderManipulation (MAC_HeaderManipulation):normalMacHeader
dl_TransportChannelType (SS_DL_TransportChannelType):bch
logicalChannelIdentity:1
logicalChannelType:bCCH

rlc_SizeList:

configured:

mac_LogicalChannelPriority:1

rB_Identity:-1
cn_DomainIdentity: Omit

#### CMAC Configuration REQ

LLA MAC @ 00:00:12.850

BTS unit: 1:2
Channel No: 0 Name: P_CCPCH
CFN: 14

Message Details:

Configuration Parameters:

Number Of Transport Channels:1

Transport Channels:

Item Number 0:

Transport Channel Parameters:

Transport Channel:

Name:BCH
Identity:0

TTI (ms):20
EP Type:1/2 Rate Convolutional Coding
CRC Size:16
RM Attribute:1
First Interleave:On
Number Of Transport Formats:2

Transport Format Set:

Transport Format 0:

Number Of Transport Blocks:0
Transport Block Size In Bits:0

Transport Format 1:

Number Of Transport Blocks:1
Transport Block Size In Bits:246

Number Of Logical Channels:1

Logical Channels:

Item Number 0:

Logical Channel:

Name:BCCH
Identity:0

Priority:1
CT Length:0
CT Value:0
TCTF Length:0
TCTF Value:0
UE ID Type:Not used
UE ID:0

Active Flag:1

Transport Format Combination Set:

Number Of Transport Format Combinations:2

Transport Format Combinations 0:

Transport Format:0

Transport Format Combinations 1:

Transport Format:1

#### CMAC Configuration CNF

MAC LLA @ 00:00:12.850

BTS unit: 1:2
Channel No: 0 Name: P_CCPCH
CFN: 14

Message Details:

#### CMAC_Config_CNF

LLA RRC @ 00:00:12.860

Channel ID: P-CCPCH
Cell ID: 3

Message Details:

CMAC_Config_CNF:

cellId:3

routingInfo:

physicalChannelIdentity:4

#### CPHY_RL_Setup_REQ

RRC LLA @ 00:00:12.860

Channel ID: S-CCPCH#1
Cell ID: 3

Message Details:

CPHY_RL_Setup_REQ:

cellId:3

routingInfo:

physicalChannelIdentity:5

ratType:fdd

setupMessage: (CphyRlSetupReq)

physicalChannelInfo:

secondaryCCPCHInfo:

scramblingCode:0

dl_ChannelizationCode: (SF256_AndCodeNumber)

sf64:1

sCCPCHSlotFormat:8
timingOffset:0
positionFixedOrFlexible:flexible
sttd_Indicator:false
dl_TxPower:-2
powerOffsetOfTFCI_PO1:6
powerOffsetOfPILOT_PO3:6

#### CPHY Radio Link Setup REQ

LLA PHY @ 00:00:13.010

BTS unit: 1:2
Channel No: 0 Name: S_CCPCH
CFN: 30

Message Details:

Configuration Parameters:

Channel Offset:7680
Scrambling Code:4000
Symbol Rate:60k
Channelization Code:1
Adjust Time:0
Power in dBm:-67
Tx Diversity:Off
Slot Format:8
NumOfDpdch:1

#### CPHY Radio Link Setup CNF

PHY LLA @ 00:00:13.010

BTS unit: 1:2
Channel No: 0 Name: S_CCPCH
CFN: 30

Message Details:

#### CPHY_RL_Setup_CNF

LLA RRC @ 00:00:13.040

Channel ID: S-CCPCH#1
Cell ID: 3

Message Details:

CPHY_RL_Setup_CNF:

cellId:3

routingInfo:

physicalChannelIdentity:5

#### CPHY_TrCH_Config_REQ

RRC LLA @ 00:00:13.040

Channel ID: S-CCPCH#1
Cell ID: 3

Message Details:

CPHY_TrCH_Config_REQ:

cellId:3

routingInfo:

physicalChannelIdentity:5

ratType:fdd

trchConfigType:

nonDch:

configMessage: (CphyTrchConfigReq)

activationTime: (SS_ActivationTime)

activateNow:

ulconnectedTrCHList: Omit

ulTFCS: (TFCS) Omit

dlconnectedTrCHList:

:

trchid (TransportChannelIdentity):12
dl_TransportChannelType (SS_DL_TransportChannelType):pch

transportChannelInfo: (CommonOrDedicatedTFS)

tti:

tti10: (CommonOrDedicatedTF_InfoList)

CommonOrDedicatedTF_Info:

tb_Size:240

numberOfTbSizeList:

NumberOfTransportBlocks:

zero:

NumberOfTransportBlocks:

one:

logicalChannelList:

allSizes:

semistaticTF_Information:

channelCodingType:

convolutional (CodingRate):half

rateMatchingAttribute:230
crc_Size:crc16

:

trchid (TransportChannelIdentity):13
dl_TransportChannelType (SS_DL_TransportChannelType):fach

transportChannelInfo: (CommonOrDedicatedTFS)

tti:

tti10: (CommonOrDedicatedTF_InfoList)

CommonOrDedicatedTF_Info:

tb_Size:168

numberOfTbSizeList:

NumberOfTransportBlocks:

zero:

NumberOfTransportBlocks:

one:

NumberOfTransportBlocks:

small:2

logicalChannelList:

allSizes:

semistaticTF_Information:

channelCodingType:

convolutional (CodingRate):half

rateMatchingAttribute:220
crc_Size:crc16

:

trchid (TransportChannelIdentity):14
dl_TransportChannelType (SS_DL_TransportChannelType):fach

transportChannelInfo: (CommonOrDedicatedTFS)

tti:

tti10: (CommonOrDedicatedTF_InfoList)

CommonOrDedicatedTF_Info:

tb_Size:360

numberOfTbSizeList:

NumberOfTransportBlocks:

zero:

NumberOfTransportBlocks:

one:

logicalChannelList:

allSizes:

semistaticTF_Information:

channelCodingType:

turbo:

rateMatchingAttribute:130
crc_Size:crc16

dlTFCS: (TFCS)

normalTFCI_Signalling: (ExplicitTFCS_Configuration)

complete: (TFCS_ReconfAdd)

ctfcSize:

ctfc4Bit:

:

ctfc4:0

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:1

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:2

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:3

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:4

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:5

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:6

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:8

powerOffsetInformation:

gainFactorInformation:

signalledGainFactors:

modeSpecificInfo:

fdd:

gainFactorBetaC (GainFactor):11

gainFactorBetaD (GainFactor):15
referenceTFC_ID:0

powerOffsetPp_m: Omit

#### CPHY Transport Channel Configuration REQ

LLA PHY @ 00:00:13.050

BTS unit: 1:2
Channel No: 0 Name: S_CCPCH
CFN: 34

Message Details:

Configuration Parameters:

DTX Position:Flexible
Second Interleave:On
Puncture Limit:100
CCTrCH Length:1080
Number Of Transport Channels:3

Transport Channels:

Item Number 0:

Transport Channel Parameters:

Transport Channel:

Name:PCH
Identity:0

TTI (ms):10
EP Type:1/2 Rate Convolutional Coding
CRC Size:16
RM Attribute:230
First Interleave:On
Number Of Transport Formats:2

Transport Format Set:

Transport Format 0:

Number Of Transport Blocks:0
Transport Block Size In Bits:240

Transport Format 1:

Number Of Transport Blocks:1
Transport Block Size In Bits:240

RM Maximum Length:457

Item Number 1:

Transport Channel Parameters:

Transport Channel:

Name:FACH
Identity:0

TTI (ms):10
EP Type:1/2 Rate Convolutional Coding
CRC Size:16
RM Attribute:220
First Interleave:On
Number Of Transport Formats:3

Transport Format Set:

Transport Format 0:

Number Of Transport Blocks:0
Transport Block Size In Bits:168

Transport Format 1:

Number Of Transport Blocks:1
Transport Block Size In Bits:168

Transport Format 2:

Number Of Transport Blocks:2
Transport Block Size In Bits:168

RM Maximum Length:623

Item Number 2:

Transport Channel Parameters:

Transport Channel:

Name:FACH
Identity:1

TTI (ms):10
EP Type:Turbo Coding
CRC Size:16
RM Attribute:130
First Interleave:On
Number Of Transport Formats:2

Transport Format Set:

Transport Format 0:

Number Of Transport Blocks:0
Transport Block Size In Bits:360

Transport Format 1:

Number Of Transport Blocks:1
Transport Block Size In Bits:360

RM Maximum Length:558

Transport Format Combination Set:

Number Of Transport Format Combinations:8

Transport Format Combinations 0:

Transport Format:0
Transport Format:0
Transport Format:0

Transport Format Combinations 1:

Transport Format:1
Transport Format:0
Transport Format:0

Transport Format Combinations 2:

Transport Format:0
Transport Format:1
Transport Format:0

Transport Format Combinations 3:

Transport Format:1
Transport Format:1
Transport Format:0

Transport Format Combinations 4:

Transport Format:0
Transport Format:2
Transport Format:0

Transport Format Combinations 5:

Transport Format:1
Transport Format:2
Transport Format:0

Transport Format Combinations 6:

Transport Format:0
Transport Format:0
Transport Format:1

Transport Format Combinations 7:

Transport Format:0
Transport Format:1
Transport Format:1

#### CPHY Transport Channel Configuration CNF

PHY LLA @ 00:00:13.050

BTS unit: 1:2
Channel No: 0 Name: S_CCPCH
CFN: 34

Message Details:

#### CPHY_TrCH_Config_CNF

LLA RRC @ 00:00:13.070

Channel ID: S-CCPCH#1
Cell ID: 3

Message Details:

CPHY_TrCH_Config_CNF:

cellId:3

routingInfo:

physicalChannelIdentity:5

#### CMAC_Config_REQ

RRC LLA @ 00:00:13.070

Channel ID: S-CCPCH#1
Cell ID: 3

Message Details:

CMAC_Config_REQ:

cellId:3

routingInfo:

physicalChannelIdentity:5

ratType:fdd

configMessage:

setup: (CmacConfigReq)

activationTime: (SS_ActivationTime)

activateNow:

uE_Info:

u_RNTI: Omit

c_RNTI: Omit

trCHInfo:

ulconnectedTrCHList: Omit

ulTFCS: (TFCS) Omit

dlconnectedTrCHList:

:

trchid (TransportChannelIdentity):12

transportChannelInfo: (CommonOrDedicatedTFS)

tti:

tti10: (CommonOrDedicatedTF_InfoList)

CommonOrDedicatedTF_Info:

tb_Size:240

numberOfTbSizeList:

NumberOfTransportBlocks:

zero:

NumberOfTransportBlocks:

one:

logicalChannelList:

allSizes:

semistaticTF_Information:

channelCodingType:

convolutional (CodingRate):half

rateMatchingAttribute:230
crc_Size:crc16

:

trchid (TransportChannelIdentity):13

transportChannelInfo: (CommonOrDedicatedTFS)

tti:

tti10: (CommonOrDedicatedTF_InfoList)

CommonOrDedicatedTF_Info:

tb_Size:168

numberOfTbSizeList:

NumberOfTransportBlocks:

zero:

NumberOfTransportBlocks:

one:

NumberOfTransportBlocks:

small:2

logicalChannelList:

allSizes:

semistaticTF_Information:

channelCodingType:

convolutional (CodingRate):half

rateMatchingAttribute:220
crc_Size:crc16

:

trchid (TransportChannelIdentity):14

transportChannelInfo: (CommonOrDedicatedTFS)

tti:

tti10: (CommonOrDedicatedTF_InfoList)

CommonOrDedicatedTF_Info:

tb_Size:360

numberOfTbSizeList:

NumberOfTransportBlocks:

zero:

NumberOfTransportBlocks:

one:

logicalChannelList:

allSizes:

semistaticTF_Information:

channelCodingType:

turbo:

rateMatchingAttribute:130
crc_Size:crc16

dlTFCS: (TFCS)

normalTFCI_Signalling: (ExplicitTFCS_Configuration)

complete: (TFCS_ReconfAdd)

ctfcSize:

ctfc4Bit:

:

ctfc4:0

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:1

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:2

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:3

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:4

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:5

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:6

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:8

powerOffsetInformation:

gainFactorInformation:

signalledGainFactors:

modeSpecificInfo:

fdd:

gainFactorBetaC (GainFactor):11

gainFactorBetaD (GainFactor):15
referenceTFC_ID:0

powerOffsetPp_m: Omit

trCH_LogCHMapping: (TrCH_LogCHMappingList1)

ulconnectedTrCHList: Omit

dlconnectedTrCHList:

:

trchid (TransportChannelIdentity):12

trCH_LogCHMappingList:

TrCH_LogicalChannelMapping:

logicalChannel_Mapping:

dl_LogicalChannelMapping: (SS_DL_LogicalChannelMapping)

macHeaderManipulation (MAC_HeaderManipulation):normalMacHeader
dl_TransportChannelType (SS_DL_TransportChannelType):pch
logicalChannelIdentity:1
logicalChannelType:pCCH

rlc_SizeList:

configured:

mac_LogicalChannelPriority:1

rB_Identity:-2
cn_DomainIdentity: Omit

:

trchid (TransportChannelIdentity):13

trCH_LogCHMappingList:

TrCH_LogicalChannelMapping:

logicalChannel_Mapping:

dl_LogicalChannelMapping: (SS_DL_LogicalChannelMapping)

macHeaderManipulation (MAC_HeaderManipulation):normalMacHeader
dl_TransportChannelType (SS_DL_TransportChannelType):fach
logicalChannelIdentity:5
logicalChannelType:cCCH

rlc_SizeList:

configured:

mac_LogicalChannelPriority:1

rB_Identity:0
cn_DomainIdentity: Omit

#### CMAC_Config_CNF

LLA RRC @ 00:00:13.080

Channel ID: S-CCPCH#1
Cell ID: 3

Message Details:

CMAC_Config_CNF:

cellId:3

routingInfo:

physicalChannelIdentity:5

#### CPHY_RL_Setup_REQ

RRC LLA @ 00:00:13.080

Channel ID: PICH#1
Cell ID: 3

Message Details:

CPHY_RL_Setup_REQ:

cellId:3

routingInfo:

physicalChannelIdentity:6

ratType:fdd

setupMessage: (CphyRlSetupReq)

physicalChannelInfo:

pICHInfo:

pichinfo: (PICH_Info)

fdd:

channelisationCode256:2
pi_CountPerFrame:e18
sttd_Indicator:false

dl_TxPower (PICH_PowerOffset):-5
sccpchId_associated:5

#### CPHY Radio Link Setup REQ

LLA PHY @ 00:00:13.190

BTS unit: 1:2
Channel No: 0 Name: PICH
CFN: 48

Message Details:

Configuration Parameters:

Channel Offset:0
Scrambling Code:4000
Symbol Rate:15k
Channelization Code:2
Adjust Time:0
Power in dBm:-70
Tx Diversity:Off
NumOfDpdch:0
Np:18

#### CPHY Radio Link Setup CNF

PHY LLA @ 00:00:13.190

BTS unit: 1:2
Channel No: 0 Name: PICH
CFN: 48

Message Details:

#### CPHY_RL_Setup_CNF

LLA RRC @ 00:00:13.220

Channel ID: PICH#1
Cell ID: 3

Message Details:

CPHY_RL_Setup_CNF:

cellId:3

routingInfo:

physicalChannelIdentity:6

#### CPHY_RL_Setup_REQ

RRC LLA @ 00:00:13.220

Channel ID: AICH#1
Cell ID: 3

Message Details:

CPHY_RL_Setup_REQ:

cellId:3

routingInfo:

physicalChannelIdentity:7

ratType:fdd

setupMessage: (CphyRlSetupReq)

physicalChannelInfo:

aICHInfo:

aichinfo: (AICH_Info)

channelisationCode256:3
sttd_Indicator:false
aich_TransmissionTiming:e0

dl_TxPower (AICH_PowerOffset):-5

#### CPHY Radio Link Setup REQ

LLA PHY @ 00:00:13.350

BTS unit: 1:2
Channel No: 0 Name: AICH
CFN: 64

Message Details:

Configuration Parameters:

Channel Offset:7680
Scrambling Code:4000
Symbol Rate:15k
Channelization Code:3
Adjust Time:0
Power in dBm:-70
Tx Diversity:Off
AICH Transmission Timing:3 Access Slots
AICH Polarity:Positive
NumOfDpdch:0

#### CPHY Radio Link Setup CNF

PHY LLA @ 00:00:13.350

BTS unit: 1:2
Channel No: 0 Name: AICH
CFN: 64

Message Details:

#### CPHY_RL_Setup_CNF

LLA RRC @ 00:00:13.360

Channel ID: AICH#1
Cell ID: 3

Message Details:

CPHY_RL_Setup_CNF:

cellId:3

routingInfo:

physicalChannelIdentity:7

#### CPHY_RL_Setup_REQ

RRC LLA @ 00:00:13.360

Channel ID: PRACH#1
Cell ID: 3

Message Details:

CPHY_RL_Setup_REQ:

cellId:3

routingInfo:

physicalChannelIdentity:8

ratType:fdd

setupMessage: (CphyRlSetupReq)

physicalChannelInfo:

pRACHInfo:

fdd_tdd:

fdd:

preambleSignature (AvailableSignatures):0000000011111111
spreadingFactorForDataPart (SF_PRACH):sfpr64
preambleScramblingCode (PreambleScramblingCodeWordNumber):0
puncturingLimit:pl1
accessSlot (AvailableSubChannelNumbers):111111111111

#### CPHY_RL_Setup_CNF

LLA RRC @ 00:00:13.380

Channel ID: PRACH#1
Cell ID: 3

Message Details:

CPHY_RL_Setup_CNF:

cellId:3

routingInfo:

physicalChannelIdentity:8

#### CPHY_TrCH_Config_REQ

RRC LLA @ 00:00:13.380

Channel ID: PRACH#1
Cell ID: 3

Message Details:

CPHY_TrCH_Config_REQ:

cellId:3

routingInfo:

physicalChannelIdentity:8

ratType:fdd

trchConfigType:

nonDch:

configMessage: (CphyTrchConfigReq)

activationTime: (SS_ActivationTime)

activateNow:

ulconnectedTrCHList:

:

trchid (TransportChannelIdentity):15
ul_TransportChannelType (SS_UL_TransportChannelType):rach

transportChannelInfo: (CommonOrDedicatedTFS)

tti:

tti20: (CommonOrDedicatedTF_InfoList)

CommonOrDedicatedTF_Info:

tb_Size:168

numberOfTbSizeList:

NumberOfTransportBlocks:

one:

logicalChannelList:

configured:

CommonOrDedicatedTF_Info:

tb_Size:360

numberOfTbSizeList:

NumberOfTransportBlocks:

one:

logicalChannelList:

configured:

semistaticTF_Information:

channelCodingType:

convolutional (CodingRate):half

rateMatchingAttribute:150
crc_Size:crc16

ulTFCS: (TFCS)

normalTFCI_Signalling: (ExplicitTFCS_Configuration)

complete: (TFCS_ReconfAdd)

ctfcSize:

ctfc2Bit:

:

ctfc2:0

powerOffsetInformation: Omit

:

ctfc2:1

powerOffsetInformation: Omit

dlconnectedTrCHList: Omit

dlTFCS: (TFCS) Omit

#### CPHY Radio Link Setup REQ

LLA PHY @ 00:00:13.430

BTS unit: 1:2
Channel No: 0 Name: PRACH
CFN: 72

Message Details:

Configuration Parameters:

Channel Offset:10240
Scrambling Code:16781216
Symbol Rate:60k
Channelization Code:128
Adjust Time:0
Slot Format:2
NumOfDpdch:1

#### CPHY Radio Link Setup CNF

PHY LLA @ 00:00:13.430

BTS unit: 1:2
Channel No: 0 Name: PRACH
CFN: 72

Message Details:

#### CPHY Transport Channel Configuration REQ

LLA PHY @ 00:00:13.460

BTS unit: 1:2
Channel No: 0 Name: PRACH
CFN: 75

Message Details:

Configuration Parameters:

DTX Position:Flexible
Second Interleave:On
Puncture Limit:100
CCTrCH Length:600
Number Of Transport Channels:1

Transport Channels:

Item Number 0:

Transport Channel Parameters:

Transport Channel:

Name:RACH
Identity:0

TTI (ms):20
EP Type:1/2 Rate Convolutional Coding
CRC Size:16
RM Attribute:150
First Interleave:On
Number Of Transport Formats:2

Transport Format Set:

Transport Format 0:

Number Of Transport Blocks:1
Transport Block Size In Bits:168

Transport Format 1:

Number Of Transport Blocks:1
Transport Block Size In Bits:360

RM Maximum Length:600

Transport Format Combination Set:

Number Of Transport Format Combinations:2

Transport Format Combinations 0:

Transport Format:0

Transport Format Combinations 1:

Transport Format:1

#### CPHY Transport Channel Configuration CNF

PHY LLA @ 00:00:13.480

BTS unit: 1:2
Channel No: 0 Name: PRACH
CFN: 77

Message Details:

#### CPHY_TrCH_Config_CNF

LLA RRC @ 00:00:13.490

Channel ID: PRACH#1
Cell ID: 3

Message Details:

CPHY_TrCH_Config_CNF:

cellId:3

routingInfo:

physicalChannelIdentity:8

#### CMAC_Config_REQ

RRC LLA @ 00:00:13.490

Channel ID: PRACH#1
Cell ID: 3

Message Details:

CMAC_Config_REQ:

cellId:3

routingInfo:

physicalChannelIdentity:8

ratType:fdd

configMessage:

setup: (CmacConfigReq)

activationTime: (SS_ActivationTime)

activateNow:

uE_Info:

u_RNTI: Omit

c_RNTI: Omit

trCHInfo:

ulconnectedTrCHList:

:

trchid (TransportChannelIdentity):15

transportChannelInfo: (CommonOrDedicatedTFS)

tti:

tti20: (CommonOrDedicatedTF_InfoList)

CommonOrDedicatedTF_Info:

tb_Size:168

numberOfTbSizeList:

NumberOfTransportBlocks:

one:

logicalChannelList:

configured:

CommonOrDedicatedTF_Info:

tb_Size:360

numberOfTbSizeList:

NumberOfTransportBlocks:

one:

logicalChannelList:

configured:

semistaticTF_Information:

channelCodingType:

convolutional (CodingRate):half

rateMatchingAttribute:150
crc_Size:crc16

ulTFCS: (TFCS)

normalTFCI_Signalling: (ExplicitTFCS_Configuration)

complete: (TFCS_ReconfAdd)

ctfcSize:

ctfc2Bit:

:

ctfc2:0

powerOffsetInformation: Omit

:

ctfc2:1

powerOffsetInformation: Omit

dlconnectedTrCHList: Omit

dlTFCS: (TFCS) Omit

trCH_LogCHMapping: (TrCH_LogCHMappingList1)

ulconnectedTrCHList:

:

trchid (TransportChannelIdentity):15

trCH_LogCHMappingList:

TrCH_LogicalChannelMapping:

logicalChannel_Mapping:

ul_LogicalChannelMapping: (SS_UL_LogicalChannelMapping)

macHeaderManipulation (MAC_HeaderManipulation):normalMacHeader
ul_TransportChannelType (SS_UL_TransportChannelType):rach
logicalChannelIdentity:5
logicalChannelType:cCCH

rB_Identity:0
cn_DomainIdentity: Omit

dlconnectedTrCHList: Omit

#### CMAC Configuration REQ

LLA MAC @ 00:00:13.510

BTS unit: 1:2
Channel No: 0 Name: PRACH
CFN: 80

Message Details:

Configuration Parameters:

Number Of Transport Channels:1

Transport Channels:

Item Number 0:

Transport Channel Parameters:

Transport Channel:

Name:RACH
Identity:0

TTI (ms):20
EP Type:1/2 Rate Convolutional Coding
CRC Size:16
RM Attribute:150
First Interleave:On
Number Of Transport Formats:2

Transport Format Set:

Transport Format 0:

Number Of Transport Blocks:1
Transport Block Size In Bits:168

Transport Format 1:

Number Of Transport Blocks:1
Transport Block Size In Bits:360

Number Of Logical Channels:1

Logical Channels:

Item Number 0:

Logical Channel:

Name:CCCH
Identity:0

Priority:0
CT Length:0
CT Value:0
TCTF Length:2
TCTF Value:0
UE ID Type:Not used
UE ID:0

Active Flag:1

Transport Format Combination Set:

Number Of Transport Format Combinations:2

Transport Format Combinations 0:

Transport Format:0

Transport Format Combinations 1:

Transport Format:1

#### CMAC Configuration CNF

MAC LLA @ 00:00:13.510

BTS unit: 1:2
Channel No: 0 Name: PRACH
CFN: 80

Message Details:

#### CMAC_Config_CNF

LLA RRC @ 00:00:13.520

Channel ID: PRACH#1
Cell ID: 3

Message Details:

CMAC_Config_CNF:

cellId:3

routingInfo:

physicalChannelIdentity:8

#### CRLC_Config_REQ

RRC LLA @ 00:00:13.520

Channel ID: RbBcch
Cell ID: 3

Message Details:

CRLC_Config_REQ:

cellId:3

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode) Omit

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):246

dl_RLCModeInfo: (UL_RLC_Mode)

ul_TM_RLC_Mode:

transmissionRLC_Discard: Omit

segmentationIndication:false

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity): Omit
dLlogicalChannelIdentity (LogicalChannelIdentity):1
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC TM Channel Establish REQ

LLA RLC @ 00:00:13.660

BTS unit: 1:2
Channel No: 0 Name: BCCH
CFN: 95

Message Details:

Configuration Parameters:

Number Of PU Sizes:1

PU sizes In Bits:

Item 0:246

#### CRLC TM Channel Establish CNF

RLC LLA @ 00:00:13.660

BTS unit: 1:2
Channel No: 0 Name: BCCH
CFN: 95

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:00:13.690

Channel ID: RbBcch
Cell ID: 3

Message Details:

CRLC_Config_CNF:

cellId:3

routingInfo:

rB_Identity:-1

#### CRLC_Config_REQ

RRC LLA @ 00:00:13.690

Channel ID: RbPcch
Cell ID: 3

Message Details:

CRLC_Config_REQ:

cellId:3

routingInfo:

rB_Identity:-2

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode) Omit

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):240

dl_RLCModeInfo: (UL_RLC_Mode)

ul_TM_RLC_Mode:

transmissionRLC_Discard: Omit

segmentationIndication:false

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity): Omit
dLlogicalChannelIdentity (LogicalChannelIdentity):1
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC TM Channel Establish REQ

LLA RLC @ 00:00:13.830

BTS unit: 1:2
Channel No: 0 Name: PCCH
CFN: 112

Message Details:

Configuration Parameters:

Number Of PU Sizes:1

PU sizes In Bits:

Item 0:240

#### CRLC TM Channel Establish CNF

RLC LLA @ 00:00:13.830

BTS unit: 1:2
Channel No: 0 Name: PCCH
CFN: 112

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:00:13.860

Channel ID: RbPcch
Cell ID: 3

Message Details:

CRLC_Config_CNF:

cellId:3

routingInfo:

rB_Identity:-2

#### CRLC_Config_REQ

RRC LLA @ 00:00:13.860

Channel ID: Rb0
Cell ID: 3

Message Details:

CRLC_Config_REQ:

cellId:3

routingInfo:

rB_Identity:0

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode) Omit

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):152

dl_RLCModeInfo: (UL_RLC_Mode)

ul_UM_RLC_Mode:

transmissionRLC_Discard:

timerBasedNoExplicit (NoExplicitDiscard):dt100

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity): Omit
dLlogicalChannelIdentity (LogicalChannelIdentity):5
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC UM Channel Establish REQ

LLA RLC @ 00:00:13.990

BTS unit: 1:2
Channel No: 1 Name: CCCH
CFN: 128

Message Details:

Configuration Parameters:

PU Size In Bits:152

#### CRLC UM Channel Establish CNF

RLC LLA @ 00:00:13.990

BTS unit: 1:2
Channel No: 1 Name: CCCH
CFN: 128

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:00:14.000

Channel ID: Rb0
Cell ID: 3

Message Details:

CRLC_Config_CNF:

cellId:3

routingInfo:

rB_Identity:0

#### CRLC_Config_REQ

RRC LLA @ 00:00:14.000

Channel ID: Rb0
Cell ID: 3

Message Details:

CRLC_Config_REQ:

cellId:3

routingInfo:

rB_Identity:0

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode)

dl_TM_RLC_Mode:

segmentationIndication:false

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):166

dl_RLCModeInfo: (UL_RLC_Mode)

ul_TM_RLC_Mode:

transmissionRLC_Discard: Omit

segmentationIndication:false

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity):5
dLlogicalChannelIdentity (LogicalChannelIdentity): Omit
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC TM Channel Establish REQ

LLA RLC @ 00:00:14.080

BTS unit: 1:2
Channel No: 0 Name: CCCH
CFN: 137

Message Details:

Configuration Parameters:

Number Of PU Sizes:1

PU sizes In Bits:

Item 0:166

#### CRLC TM Channel Establish CNF

RLC LLA @ 00:00:14.080

BTS unit: 1:2
Channel No: 0 Name: CCCH
CFN: 137

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:00:14.110

Channel ID: Rb0
Cell ID: 3

Message Details:

CRLC_Config_CNF:

cellId:3

routingInfo:

rB_Identity:0

#### o_SIB_PER_Encoding

RRC RRC @ 00:00:14.150

Category: TSO

Message Details:

Inputs:

SIB:

sIB1: (SysInfoType1)

cn_CommonGSM_MAP_NAS_SysInfo (NAS_SystemInformationGSM_MAP):

[0]00 01

cn_DomainSysInfoList:

CN_DomainSysInfo:

cn_DomainIdentity:ps_domain

cn_Type:

gsm_MAP (NAS_SystemInformationGSM_MAP):

[0]05 00

cn_DRX_CycleLengthCoeff (CN_DRX_CycleLengthCoefficient):7

CN_DomainSysInfo:

cn_DomainIdentity:cs_domain

cn_Type:

gsm_MAP (NAS_SystemInformationGSM_MAP):

[0]1E 01

cn_DRX_CycleLengthCoeff (CN_DRX_CycleLengthCoefficient):7

ue_ConnTimersAndConstants:

t_301: Omit
n_301: Omit
t_302: Omit
n_302: Omit
t_304: Omit
n_304: Omit
t_305: Omit
t_307: Omit
t_308: Omit
t_309: Omit
t_310: Omit
n_310: Omit
t_311: Omit
t_312: Omit
n_312: Omit
t_313: Omit
n_313: Omit
t_314: Omit
t_315: Omit
n_315: Omit
t_316: Omit
t_317: Omit

ue_IdleTimersAndConstants:

t_300:ms4000
n_300:3
t_312:10
n_312:s1

v3a0NonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]11 00 01 00 00 00 00 00
[8]00 00 01 01 10 00 10 00
[16]00 10 10 00 00 00 00 10
[24]00 01 00 01 11 10 00 00
[32]00 01 01 00 00 00 00 00
[40]00 00 00 00 00 00 11 00
[48]01 11 01 00 00

#### o_SIB_PER_Encoding

RRC RRC @ 00:00:14.150

Category: TSO

Message Details:

Inputs:

SIB:

sIB2: (SysInfoType2)

ura_IdentityList:

URA_Identity:0000000000000010

nonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]00 00 00 00 00 00 00 00
[8]00 10

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:00:14.150

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:3

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:10
bcch_ModificationTime: Omit

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:00:14.160

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:3

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:00:14.160

Channel ID: RbBcch
Cell ID: 3

Message Details:

RLC_TR_DATA_REQ:

cellId:3

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

completeSIB_List:

CompleteSIBshort:

sib_Type:systemInformationBlockType1
sib_Data_variable:1100010000000000000001011000100000101000000000100001000111100000000101000000000000000000000011000111010000

CompleteSIBshort:

sib_Type:systemInformationBlockType2
sib_Data_variable:00000000000000000010

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:00:14.160

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 20

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

completeSIB_List:

CompleteSIB_List.element:

sib_Type: systemInformationBlockType1_SIB_Type [enum=1]

sib_Data_variable: 1100010000000000000001011000100000101000000000100001000111100000000101000000000000000000000011000111010000

CompleteSIB_List.element:

sib_Type: systemInformationBlockType2_SIB_Type [enum=2]

sib_Data_variable: 00000000000000000010

Layer 3 SDU:

[0]00 0E 21 69 C4 00 05 88
[8]28 02 11 E0 14 00 00 0C
[16]74 04 26 00 00 40

#### o_SIB_PER_Encoding

RRC RRC @ 00:00:14.160

Category: TSO

Message Details:

Inputs:

SIB:

sIB2: (SysInfoType2)

ura_IdentityList:

URA_Identity:0000000000000010

nonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]00 00 00 00 00 00 00 00
[8]00 10

#### o_SIB_PER_Encoding

RRC RRC @ 00:00:14.160

Category: TSO

Message Details:

Inputs:

SIB:

sIB1: (SysInfoType1)

cn_CommonGSM_MAP_NAS_SysInfo (NAS_SystemInformationGSM_MAP):

[0]00 01

cn_DomainSysInfoList:

CN_DomainSysInfo:

cn_DomainIdentity:ps_domain

cn_Type:

gsm_MAP (NAS_SystemInformationGSM_MAP):

[0]05 00

cn_DRX_CycleLengthCoeff (CN_DRX_CycleLengthCoefficient):7

CN_DomainSysInfo:

cn_DomainIdentity:cs_domain

cn_Type:

gsm_MAP (NAS_SystemInformationGSM_MAP):

[0]1E 01

cn_DRX_CycleLengthCoeff (CN_DRX_CycleLengthCoefficient):7

ue_ConnTimersAndConstants:

t_301: Omit
n_301: Omit
t_302: Omit
n_302: Omit
t_304: Omit
n_304: Omit
t_305: Omit
t_307: Omit
t_308: Omit
t_309: Omit
t_310: Omit
n_310: Omit
t_311: Omit
t_312: Omit
n_312: Omit
t_313: Omit
n_313: Omit
t_314: Omit
t_315: Omit
n_315: Omit
t_316: Omit
t_317: Omit

ue_IdleTimersAndConstants:

t_300:ms4000
n_300:3
t_312:10
n_312:s1

v3a0NonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]11 00 01 00 00 00 00 00
[8]00 00 01 01 10 00 10 00
[16]00 10 10 00 00 00 00 10
[24]00 01 00 01 11 10 00 00
[32]00 01 01 00 00 00 00 00
[40]00 00 00 00 00 00 11 00
[48]01 11 01 00 00

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:00:14.160

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:3

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:10
bcch_ModificationTime: Omit

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:00:14.180

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:3

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:00:14.180

Channel ID: RbBcch
Cell ID: 3

Message Details:

RLC_TR_DATA_REQ:

cellId:3

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

completeSIB_List:

CompleteSIBshort:

sib_Type:systemInformationBlockType1
sib_Data_variable:1100010000000000000001011000100000101000000000100001000111100000000101000000000000000000000011000111010000

CompleteSIBshort:

sib_Type:systemInformationBlockType2
sib_Data_variable:00000000000000000010

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:00:14.180

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 20

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

completeSIB_List:

CompleteSIB_List.element:

sib_Type: systemInformationBlockType1_SIB_Type [enum=1]

sib_Data_variable: 1100010000000000000001011000100000101000000000100001000111100000000101000000000000000000000011000111010000

CompleteSIB_List.element:

sib_Type: systemInformationBlockType2_SIB_Type [enum=2]

sib_Data_variable: 00000000000000000010

Layer 3 SDU:

[0]00 0E 21 69 C4 00 05 88
[8]28 02 11 E0 14 00 00 0C
[16]74 04 26 00 00 40

#### o_SIB_PER_Encoding

RRC RRC @ 00:00:14.180

Category: TSO

Message Details:

Inputs:

SIB:

sIB3: (SysInfoType3)

sib4indicator:true
cellIdentity:0000000000000000000000000011

cellSelectReselectInfo: (CellSelectReselectInfoSIB_3_4)

mappingInfo: Omit

cellSelectQualityMeasure:

cpich_RSCP:

modeSpecificInfo:

fdd:

s_Intrasearch (S_SearchQual):8
s_Intersearch (S_SearchQual):8
s_SearchHCS (S_SearchRXLEV): Omit

rat_List: (RAT_FDD_InfoList)

RAT_FDD_Info:

rat_Identifier:gsm
s_SearchRAT (S_SearchQual):-16
s_HCS_RAT (S_SearchRXLEV): Omit
s_Limit_SearchRAT (S_SearchQual):0

q_QualMin:-24
q_RxlevMin:-40

q_Hyst_l_S (Q_Hyst_S):2
t_Reselection_S:0

hcs_ServingCellInformation: Omit

maxAllowedUL_TX_Power:21

cellAccessRestriction:

cellBarred:

notBarred:

cellReservedForOperatorUse (ReservedIndicator):notReserved
cellReservationExtension (ReservedIndicator):notReserved

accessClassBarredList:

AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred

nonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]01 00 00 00 00 00 00 00
[8]00 00 00 00 00 00 11 00
[16]10 11 01 11 00 01 10 00
[24]00 00 00 00 00 01 00 00
[32]00 00 00 10 01 00 00 10
[40]00 00 01 00 01 11 11 11
[48]11 11 11 11 11 11 11 11

#### o_SIB_PER_Encoding

RRC RRC @ 00:00:14.180

Category: TSO

Message Details:

Inputs:

SIB:

sIB7: (SysInfoType7)

modeSpecificInfo:

fdd:

ul_Interference:-100

prach_Information_SIB5_List: (DynamicPersistenceLevelList)

DynamicPersistenceLevel:2

prach_Information_SIB6_List: (DynamicPersistenceLevelList)

DynamicPersistenceLevel:2

expirationTimeFactor: Omit

nonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]10 00 00 10 10 00 00 00
[8]10 00 00 01

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:00:14.180

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:3

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:7
bcch_ModificationTime: Omit

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:00:14.190

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:3

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:00:14.190

Channel ID: RbBcch
Cell ID: 3

Message Details:

RLC_TR_DATA_REQ:

cellId:3

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

completeSIB_List:

CompleteSIBshort:

sib_Type:systemInformationBlockType7
sib_Data_variable:100000101000000010000001

CompleteSIBshort:

sib_Type:systemInformationBlockType3
sib_Data_variable:0100000000000000000000000000110010110111000110000000000000010000000000100100001000000100011111111111111111111111

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:00:14.190

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 14

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

completeSIB_List:

CompleteSIB_List.element:

sib_Type: systemInformationBlockType7_SIB_Type [enum=7]

sib_Data_variable: 100000101000000010000001

CompleteSIB_List.element:

sib_Type: systemInformationBlockType3_SIB_Type [enum=3]

sib_Data_variable: 0100000000000000000000000000110010110111000110000000000000010000000000100100001000000100011111111111111111111111

Layer 3 SDU:

[0]00 0E 27 17 82 80 81 1B
[8]7A 00 00 00 65 B8 C0 00
[16]80 12 10 23 FF FF F8

#### o_SIB_PER_Encoding

RRC RRC @ 00:00:14.190

Category: TSO

Message Details:

Inputs:

SIB:

sIB4: (SysInfoType4)

cellIdentity:0000000000000000000000000011

cellSelectReselectInfo: (CellSelectReselectInfoSIB_3_4)

mappingInfo: Omit

cellSelectQualityMeasure:

cpich_RSCP:

modeSpecificInfo:

fdd:

s_Intrasearch (S_SearchQual):8
s_Intersearch (S_SearchQual):8
s_SearchHCS (S_SearchRXLEV): Omit

rat_List: (RAT_FDD_InfoList)

RAT_FDD_Info:

rat_Identifier:gsm
s_SearchRAT (S_SearchQual):-16
s_HCS_RAT (S_SearchRXLEV): Omit
s_Limit_SearchRAT (S_SearchQual):0

q_QualMin:-24
q_RxlevMin:-40

q_Hyst_l_S (Q_Hyst_S):0
t_Reselection_S:0

hcs_ServingCellInformation: Omit

maxAllowedUL_TX_Power:21

cellAccessRestriction:

cellBarred:

notBarred:

cellReservedForOperatorUse (ReservedIndicator):notReserved
cellReservationExtension (ReservedIndicator):notReserved

accessClassBarredList: Omit

nonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]00 00 00 00 00 00 00 00
[8]00 00 00 00 00 01 10 01
[16]01 10 11 10 00 11 00 00
[24]00 00 00 00 00 10 00 00
[32]00 00 01 00 10 00 00 00
[40]00 00 10 00 11 10 11 1

#### o_SIB_PER_Encoding

RRC RRC @ 00:00:14.190

Category: TSO

Message Details:

Inputs:

SIB:

sIB7: (SysInfoType7)

modeSpecificInfo:

fdd:

ul_Interference:-100

prach_Information_SIB5_List: (DynamicPersistenceLevelList)

DynamicPersistenceLevel:2

prach_Information_SIB6_List: (DynamicPersistenceLevelList)

DynamicPersistenceLevel:2

expirationTimeFactor: Omit

nonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]10 00 00 10 10 00 00 00
[8]10 00 00 01

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:00:14.190

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:3

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:31
bcch_ModificationTime: Omit

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:00:14.210

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:3

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:00:14.210

Channel ID: RbBcch
Cell ID: 3

Message Details:

RLC_TR_DATA_REQ:

cellId:3

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

completeSIB_List:

CompleteSIBshort:

sib_Type:systemInformationBlockType7
sib_Data_variable:100000101000000010000001

CompleteSIBshort:

sib_Type:systemInformationBlockType4
sib_Data_variable:00000000000000000000000000011001011011100011000000000000001000000000010010000000000010001110111

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:00:14.210

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 62

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

completeSIB_List:

CompleteSIB_List.element:

sib_Type: systemInformationBlockType7_SIB_Type [enum=7]

sib_Data_variable: 100000101000000010000001

CompleteSIB_List.element:

sib_Type: systemInformationBlockType4_SIB_Type [enum=4]

sib_Data_variable: 00000000000000000000000000011001011011100011000000000000001000000000010010000000000010001110111

Layer 3 SDU:

[0]00 0E 27 17 82 80 81 22
[8]F0 00 00 00 CB 71 80 01
[16]00 24 00 47 70

#### o_SIB_PER_Encoding

RRC RRC @ 00:00:14.220

Category: TSO

Message Details:

Inputs:

SIB:

sIB5: (SysInfoType5)

sib6indicator:true
pich_PowerOffset:-5

modeSpecificInfo:

fdd:

aich_PowerOffset:-5

primaryCCPCH_Info: Omit

prach_SystemInformationList:

PRACH_SystemInformation:

prach_RACH_Info:

modeSpecificInfo:

fdd:

availableSignatures:0000000011111111
availableSF (SF_PRACH):sfpr64
preambleScramblingCodeWordNumber:0
puncturingLimit:pl1
availableSubChannelNumbers:111111111111

transportChannelIdentity:15

rach_TransportFormatSet: (TransportFormatSet)

commonTransChTFS:

tti:

tti20: (CommonDynamicTF_InfoList)

CommonDynamicTF_Info:

rlc_Size:

fdd:

octetModeRLC_SizeInfoType2:

sizeType1:15

numberOfTbSizeList:

NumberOfTransportBlocks:

one:

logicalChannelList:

configured:

CommonDynamicTF_Info:

rlc_Size:

fdd:

octetModeRLC_SizeInfoType2:

sizeType2:3

numberOfTbSizeList:

NumberOfTransportBlocks:

one:

logicalChannelList:

configured:

semistaticTF_Information:

channelCodingType:

convolutional (CodingRate):half

rateMatchingAttribute:150
crc_Size:crc16

rach_TFCS: (TFCS)

normalTFCI_Signalling: (ExplicitTFCS_Configuration)

complete: (TFCS_ReconfAdd)

ctfcSize:

ctfc2Bit:

:

ctfc2:0

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m:0

:

ctfc2:1

powerOffsetInformation:

gainFactorInformation:

signalledGainFactors:

modeSpecificInfo:

fdd:

gainFactorBetaC (GainFactor):11

gainFactorBetaD (GainFactor):15
referenceTFC_ID:0

powerOffsetPp_m:0

prach_Partitioning:

fdd:

ASCSetting_FDD:

accessServiceClass_FDD: Omit

ASCSetting_FDD:

accessServiceClass_FDD:

availableSignatureStartIndex:0
availableSignatureEndIndex:7
assignedSubChannelNumber:1111

ASCSetting_FDD:

accessServiceClass_FDD: Omit

ASCSetting_FDD:

accessServiceClass_FDD:

availableSignatureStartIndex:0
availableSignatureEndIndex:7
assignedSubChannelNumber:1111

ASCSetting_FDD:

accessServiceClass_FDD: Omit

ASCSetting_FDD:

accessServiceClass_FDD:

availableSignatureStartIndex:0
availableSignatureEndIndex:7
assignedSubChannelNumber:1111

ASCSetting_FDD:

accessServiceClass_FDD: Omit

ASCSetting_FDD:

accessServiceClass_FDD:

availableSignatureStartIndex:0
availableSignatureEndIndex:7
assignedSubChannelNumber:1111

persistenceScalingFactorList:

PersistenceScalingFactor:psf0_9
PersistenceScalingFactor:psf0_9
PersistenceScalingFactor:psf0_9
PersistenceScalingFactor:psf0_9
PersistenceScalingFactor:psf0_9
PersistenceScalingFactor:psf0_9

ac_To_ASC_MappingTable:

AC_To_ASC_Mapping:6
AC_To_ASC_Mapping:5
AC_To_ASC_Mapping:4
AC_To_ASC_Mapping:3
AC_To_ASC_Mapping:2
AC_To_ASC_Mapping:1
AC_To_ASC_Mapping:0

modeSpecificInfo:

fdd:

primaryCPICH_TX_Power:31
constantValue:-10

prach_PowerOffset:

powerRampStep:3
preambleRetransMax:4

rach_TransmissionParameters:

mmax:2
nb01Min (NB01):3
nb01Max (NB01):10

aich_Info:

channelisationCode256:3
sttd_Indicator:false
aich_TransmissionTiming:e0

sCCPCH_SystemInformationList:

SCCPCH_SystemInformation:

secondaryCCPCH_Info:

modeSpecificInfo:

fdd:

dummy1 (PCPICH_UsageForChannelEst):mayBeUsed

dummy2: (SecondaryCPICH_Info) Omit

secondaryScramblingCode: Omit
sttd_Indicator:false

sf_AndCodeNumber: (SF256_AndCodeNumber)

sf64:1

pilotSymbolExistence:false
tfci_Existence:true
positionFixedOrFlexible:flexible
timingOffset:0

tfcs:

normalTFCI_Signalling: (ExplicitTFCS_Configuration)

complete: (TFCS_ReconfAdd)

ctfcSize:

ctfc4Bit:

:

ctfc4:0

powerOffsetInformation: Omit

:

ctfc4:1

powerOffsetInformation: Omit

:

ctfc4:2

powerOffsetInformation: Omit

:

ctfc4:3

powerOffsetInformation: Omit

:

ctfc4:4

powerOffsetInformation: Omit

:

ctfc4:5

powerOffsetInformation: Omit

:

ctfc4:6

powerOffsetInformation: Omit

:

ctfc4:8

powerOffsetInformation: Omit

fach_PCH_InformationList:

FACH_PCH_Information:

transportFormatSet:

commonTransChTFS:

tti:

tti10: (CommonDynamicTF_InfoList)

CommonDynamicTF_Info:

rlc_Size:

fdd:

octetModeRLC_SizeInfoType2:

sizeType1:24

numberOfTbSizeList:

NumberOfTransportBlocks:

zero:

NumberOfTransportBlocks:

one:

logicalChannelList:

allSizes:

semistaticTF_Information:

channelCodingType:

convolutional (CodingRate):half

rateMatchingAttribute:230
crc_Size:crc16

transportChannelIdentity:12
ctch_Indicator:false

FACH_PCH_Information:

transportFormatSet:

commonTransChTFS:

tti:

tti10: (CommonDynamicTF_InfoList)

CommonDynamicTF_Info:

rlc_Size:

fdd:

octetModeRLC_SizeInfoType2:

sizeType1:15

numberOfTbSizeList:

NumberOfTransportBlocks:

zero:

NumberOfTransportBlocks:

one:

NumberOfTransportBlocks:

small:2

logicalChannelList:

allSizes:

semistaticTF_Information:

channelCodingType:

convolutional (CodingRate):half

rateMatchingAttribute:220
crc_Size:crc16

transportChannelIdentity:13
ctch_Indicator:false

FACH_PCH_Information:

transportFormatSet:

commonTransChTFS:

tti:

tti10: (CommonDynamicTF_InfoList)

CommonDynamicTF_Info:

rlc_Size:

fdd:

octetModeRLC_SizeInfoType2:

sizeType2:3

numberOfTbSizeList:

NumberOfTransportBlocks:

zero:

NumberOfTransportBlocks:

one:

logicalChannelList:

allSizes:

semistaticTF_Information:

channelCodingType:

turbo:

rateMatchingAttribute:130
crc_Size:crc16

transportChannelIdentity:14
ctch_Indicator:false

pich_Info:

fdd:

channelisationCode256:2
pi_CountPerFrame:e18
sttd_Indicator:false

cbs_DRX_Level1Information: Omit

nonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]00 01 01 01 01 00 01 00
[8]00 11 11 10 00 00 00 00
[16]11 11 11 11 01 00 00 11
[24]11 11 11 11 11 11 11 01
[32]11 01 00 10 00 01 00 00
[40]11 11 00 00 00 10 10 01
[48]00 00 11 00 00 00 10 10
[56]10 10 01 01 01 01 10 00
[64]00 00 00 00 00 00 11 00
[72]11 00 01 01 10 11 01 01
[80]01 11 11 10 00 10 10 11
[88]10 10 00 00 11 11 11 10
[96]10 00 00 11 11 11 10 10
[104]00 00 11 11 11 10 10 00
[112]00 11 11 11 11 01 00 00
[120]00 00 00 00 00 00 00 11
[128]01 01 10 00 11 01 00 01
[136]00 00 11 11 11 01 00 11
[144]10 01 01 00 00 01 10 00
[152]01 00 00 11 00 10 10 00
[160]00 00 11 00 00 00 11 10
[168]00 00 01 00 00 00 01 01
[176]10 00 00 10 00 00 00 11
[184]10 00 00 00 00 10 00 10
[192]00 01 10 01 00 00 10 10
[200]01 10 01 00 00 10 10 00
[208]00 00 00 00 11 00 00 00
[216]01 00 01 00 01 01 11 00
[224]10 10 11 01 01 10 10 00
[232]00 00 00 00 01 11 10 00
[240]10 00 01 10 00 00 00 01
[248]01 10 11 01 10 11 01 10
[256]00 10 00 00 00 00 01 00
[264]00 11 00 00 10 00 10 01
[272]01 00 00 00 10 11 01 10
[280]10 00 00 00 01 00 00

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:00:14.240

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:3

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:22
bcch_ModificationTime: Omit

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:00:14.250

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:3

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:00:14.250

Channel ID: RbBcch
Cell ID: 3

Message Details:

RLC_TR_DATA_REQ:

cellId:3

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

noSegment:

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:00:14.250

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 44

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

noSegment: NULL

Layer 3 SDU:

[0]00 00

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:00:14.250

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:3

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:18
bcch_ModificationTime: Omit

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:00:14.270

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:3

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:00:14.270

Channel ID: RbBcch
Cell ID: 3

Message Details:

RLC_TR_DATA_REQ:

cellId:3

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

firstSegment:

sib_Type:systemInformationBlockType5
seg_Count (SegCount):3
sib_Data_fixed:000101010100010000111110000000001111111101000011111111111111110111010010000100001111000000101001000011000000101010100101010110000000000000001100110001011011010101111110001010111010000011111110100000111111101000001111111010

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:00:14.270

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 36

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

firstSegment:

sib_Type: systemInformationBlockType5_SIB_Type [enum=5]

seg_Count: 3

sib_Data_fixed: 000101010100010000111110000000001111111101000011111111111111110111010010000100001111000000101001000011000000101010100101010110000000000000001100110001011011010101111110001010111010000011111110100000111111101000001111111010

Layer 3 SDU:

[0]00 02 52 15 44 3E 00 FF
[8]43 FF FD D2 10 F0 29 0C
[16]0A A5 58 00 0C C5 B5 7E
[24]2B A0 FE 83 FA 0F E8

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:00:14.270

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:3

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:19
bcch_ModificationTime: Omit

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:00:14.290

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:3

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:00:14.290

Channel ID: RbBcch
Cell ID: 3

Message Details:

RLC_TR_DATA_REQ:

cellId:3

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

subsequentSegment:

sib_Type:systemInformationBlockType5
segmentIndex:1
sib_Data_fixed:000011111111010000000000000000001101011000110100010000111111010011100101000001100001000011001010000000110000001110000001000000010110000010000000111000000000100010000110010000101001100100001010000000000011000000010001000101

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:00:14.290

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 38

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

subsequentSegment:

sib_Type: systemInformationBlockType5_SIB_Type [enum=5]

segmentIndex: 1

sib_Data_fixed: 000011111111010000000000000000001101011000110100010000111111010011100101000001100001000011001010000000110000001110000001000000010110000010000000111000000000100010000110010000101001100100001010000000000011000000010001000101

Layer 3 SDU:

[0]00 04 50 0F F4 00 00 D6
[8]34 43 F4 E5 06 10 CA 03
[16]03 81 01 60 80 E0 08 86
[24]42 99 0A 00 30 11 14

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:00:14.290

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:3

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:21
bcch_ModificationTime: Omit

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:00:14.300

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:3

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:00:14.300

Channel ID: RbBcch
Cell ID: 3

Message Details:

RLC_TR_DATA_REQ:

cellId:3

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

lastSegmentShort:

sib_Type:systemInformationBlockType5
segmentIndex:2
sib_Data_variable:1100101011010110100000000000011110001000011000000001011011011011011000100000000001000011000010001001010000001011011010000000010000

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:00:14.300

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 42

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

lastSegmentShort:

sib_Type: systemInformationBlockType5_SIB_Type [enum=5]

segmentIndex: 2

sib_Data_variable: 1100101011010110100000000000011110001000011000000001011011011011011000100000000001000011000010001001010000001011011010000000010000

Layer 3 SDU:

[0]00 06 51 81 CA D6 80 07
[8]88 60 16 DB 62 00 43 08
[16]94 0B 68 04 00

#### o_SIB_PER_Encoding

RRC RRC @ 00:00:14.300

Category: TSO

Message Details:

Inputs:

SIB:

sIB6: (SysInfoType6)

pich_PowerOffset:-5

modeSpecificInfo:

fdd:

aich_PowerOffset:-5
dummy (CSICH_PowerOffset): Omit

primaryCCPCH_Info: Omit

prach_SystemInformationList: Omit

sCCPCH_SystemInformationList: Omit

cbs_DRX_Level1Information: Omit

nonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]00 00 00 10 10 01 00 01

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:00:14.300

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:3

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:2
bcch_ModificationTime: Omit

#### MAC_DATA_REQ

RLC MAC @ 00:00:14.310

Category: Configuration
BTS unit: 1:2
Channel No: 0 Name: BCCH
CFN: 160

Message Details:

RLC PDU size (bits):176
RLC PDU (raw):

[0]00 0E 21 69 C4 00 05 88
[8]28 02 11 E0 14 00 00 0C
[16]74 04 26 00 00 40

#### MAC_DATA_REQ

RLC MAC @ 00:00:14.310

Category: Configuration
BTS unit: 1:2
Channel No: 0 Name: BCCH
CFN: 160

Message Details:

RLC PDU size (bits):176
RLC PDU (raw):

[0]00 0E 21 69 C4 00 05 88
[8]28 02 11 E0 14 00 00 0C
[16]74 04 26 00 00 40

#### MAC_DATA_REQ

RLC MAC @ 00:00:14.310

Category: Configuration
BTS unit: 1:2
Channel No: 0 Name: BCCH
CFN: 160

Message Details:

RLC PDU size (bits):184
RLC PDU (raw):

[0]00 0E 27 17 82 80 81 1B
[8]7A 00 00 00 65 B8 C0 00
[16]80 12 10 23 FF FF F8

#### MAC_DATA_REQ

RLC MAC @ 00:00:14.310

Category: Configuration
BTS unit: 1:2
Channel No: 0 Name: BCCH
CFN: 160

Message Details:

RLC PDU size (bits):168
RLC PDU (raw):

[0]00 0E 27 17 82 80 81 22
[8]F0 00 00 00 CB 71 80 01
[16]00 24 00 47 70

#### MAC_DATA_REQ

RLC MAC @ 00:00:14.310

Category: Configuration
BTS unit: 1:2
Channel No: 0 Name: BCCH
CFN: 160

Message Details:

RLC PDU size (bits):16
RLC PDU (raw):

[0]00 00

#### MAC_DATA_REQ

RLC MAC @ 00:00:14.310

Category: Configuration
BTS unit: 1:2
Channel No: 0 Name: BCCH
CFN: 160

Message Details:

RLC PDU size (bits):248
RLC PDU (raw):

[0]00 02 52 15 44 3E 00 FF
[8]43 FF FD D2 10 F0 29 0C
[16]0A A5 58 00 0C C5 B5 7E
[24]2B A0 FE 83 FA 0F E8

#### MAC_DATA_REQ

RLC MAC @ 00:00:14.310

Category: Configuration
BTS unit: 1:2
Channel No: 0 Name: BCCH
CFN: 160

Message Details:

RLC PDU size (bits):248
RLC PDU (raw):

[0]00 04 50 0F F4 00 00 D6
[8]34 43 F4 E5 06 10 CA 03
[16]03 81 01 60 80 E0 08 86
[24]42 99 0A 00 30 11 14

#### PHY_DATA_REQ

MAC PHY @ 00:00:14.310

BTS unit: 1:2
Channel No: 0 Name: BCH
CFN: 160

Message Details:

SIB repetition period:64
SIB position:20
SIB size:246
SIB (raw):

[0]00 0E 21 69 C4 00 05 88
[8]28 02 11 E0 14 00 00 0C
[16]74 04 26 00 00 40 21 01
[24]04 A1 4A 86 12 88 28 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 0E 21 69 C4 00 05 88
[8]28 02 11 E0 14 00 00 0C
[16]74 04 26 00 00 40 21 01
[24]04 A1 4A 86 12 88 28

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:00:14.320

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:3

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:00:14.320

Channel ID: RbBcch
Cell ID: 3

Message Details:

RLC_TR_DATA_REQ:

cellId:3

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

completeSIB_List:

CompleteSIBshort:

sib_Type:systemInformationBlockType6
sib_Data_variable:0000001010010001

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:00:14.320

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 4

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

completeSIB_List:

CompleteSIB_List.element:

sib_Type: systemInformationBlockType6_SIB_Type [enum=6]

sib_Data_variable: 0000001010010001

Layer 3 SDU:

[0]00 0E 06 0F 02 91

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:00:14.320

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:3

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:3
bcch_ModificationTime: Omit

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:00:14.330

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:3

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:00:14.330

Channel ID: RbBcch
Cell ID: 3

Message Details:

RLC_TR_DATA_REQ:

cellId:3

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

noSegment:

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:00:14.330

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 6

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

noSegment: NULL

Layer 3 SDU:

[0]00 00

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:00:14.330

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:3

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:5
bcch_ModificationTime: Omit

#### PHY_DATA_REQ

MAC PHY @ 00:00:14.330

BTS unit: 1:2
Channel No: 0 Name: BCH
CFN: 162

Message Details:

SIB repetition period:64
SIB position:20
SIB size:246
SIB (raw):

[0]00 0E 21 69 C4 00 05 88
[8]28 02 11 E0 14 00 00 0C
[16]74 04 26 00 00 40 21 01
[24]04 A1 4A 86 12 88 28 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 0E 21 69 C4 00 05 88
[8]28 02 11 E0 14 00 00 0C
[16]74 04 26 00 00 40 21 01
[24]04 A1 4A 86 12 88 28

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:00:14.350

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:3

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:00:14.350

Channel ID: RbBcch
Cell ID: 3

Message Details:

RLC_TR_DATA_REQ:

cellId:3

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

noSegment:

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:00:14.350

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 10

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

noSegment: NULL

Layer 3 SDU:

[0]00 00

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:00:14.350

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:3

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:6
bcch_ModificationTime: Omit

#### PHY_DATA_REQ

MAC PHY @ 00:00:14.350

BTS unit: 1:2
Channel No: 0 Name: BCH
CFN: 164

Message Details:

SIB repetition period:64
SIB position:14
SIB size:246
SIB (raw):

[0]00 0E 27 17 82 80 81 1B
[8]7A 00 00 00 65 B8 C0 00
[16]80 12 10 23 FF FF F8 01
[24]04 A1 4A 86 12 88 28 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 0E 27 17 82 80 81 1B
[8]7A 00 00 00 65 B8 C0 00
[16]80 12 10 23 FF FF F8 01
[24]04 A1 4A 86 12 88 28

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:00:14.360

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:3

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:00:14.360

Channel ID: RbBcch
Cell ID: 3

Message Details:

RLC_TR_DATA_REQ:

cellId:3

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

noSegment:

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:00:14.360

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 12

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

noSegment: NULL

Layer 3 SDU:

[0]00 00

#### o_SIB_PER_Encoding

RRC RRC @ 00:00:14.360

Category: TSO

Message Details:

Inputs:

SIB:

sIB7: (SysInfoType7)

modeSpecificInfo:

fdd:

ul_Interference:-100

prach_Information_SIB5_List: (DynamicPersistenceLevelList)

DynamicPersistenceLevel:2

prach_Information_SIB6_List: (DynamicPersistenceLevelList)

DynamicPersistenceLevel:2

expirationTimeFactor: Omit

nonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]10 00 00 10 10 00 00 00
[8]10 00 00 01

#### o_SIB_PER_Encoding

RRC RRC @ 00:00:14.360

Category: TSO

Message Details:

Inputs:

SIB:

sIB12: (SysInfoType12)

fach_MeasurementOccasionInfo: Omit

measurementControlSysInfo:

use_of_HCS:

hcs_not_used:

cellSelectQualityMeasure:

cpich_RSCP:

intraFreqMeasurementSysInfo: (IntraFreqMeasurementSysInfo_RSCP) Omit

interFreqMeasurementSysInfo: (InterFreqMeasurementSysInfo_RSCP) Omit

interRATMeasurementSysInfo: (InterRATMeasurementSysInfo_B) Omit

trafficVolumeMeasSysInfo: Omit

dummy: (UE_InternalMeasurementSysInfo) Omit

nonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]00 00 00 00 0

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:00:14.360

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:3

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:15
bcch_ModificationTime: Omit

#### PHY_DATA_REQ

MAC PHY @ 00:00:14.370

BTS unit: 1:2
Channel No: 0 Name: BCH
CFN: 166

Message Details:

SIB repetition period:64
SIB position:62
SIB size:246
SIB (raw):

[0]00 0E 27 17 82 80 81 22
[8]F0 00 00 00 CB 71 80 01
[16]00 24 00 47 70 FF F8 01
[24]04 A1 4A 86 12 88 28 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 0E 27 17 82 80 81 22
[8]F0 00 00 00 CB 71 80 01
[16]00 24 00 47 70 FF F8 01
[24]04 A1 4A 86 12 88 28

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:00:14.380

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:3

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:00:14.380

Channel ID: RbBcch
Cell ID: 3

Message Details:

RLC_TR_DATA_REQ:

cellId:3

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

completeSIB_List:

CompleteSIBshort:

sib_Type:systemInformationBlockType7
sib_Data_variable:100000101000000010000001

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:00:14.380

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 30

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

completeSIB_List:

CompleteSIB_List.element:

sib_Type: systemInformationBlockType7_SIB_Type [enum=7]

sib_Data_variable: 100000101000000010000001

Layer 3 SDU:

[0]00 0E 07 17 82 80 81

#### o_SIB_PER_Encoding

RRC RRC @ 00:00:14.380

Category: TSO

Message Details:

Inputs:

SIB:

sIB3: (SysInfoType3)

sib4indicator:true
cellIdentity:0000000000000000000000000011

cellSelectReselectInfo: (CellSelectReselectInfoSIB_3_4)

mappingInfo: Omit

cellSelectQualityMeasure:

cpich_RSCP:

modeSpecificInfo:

fdd:

s_Intrasearch (S_SearchQual):8
s_Intersearch (S_SearchQual):8
s_SearchHCS (S_SearchRXLEV): Omit

rat_List: (RAT_FDD_InfoList)

RAT_FDD_Info:

rat_Identifier:gsm
s_SearchRAT (S_SearchQual):-16
s_HCS_RAT (S_SearchRXLEV): Omit
s_Limit_SearchRAT (S_SearchQual):0

q_QualMin:-24
q_RxlevMin:-40

q_Hyst_l_S (Q_Hyst_S):2
t_Reselection_S:0

hcs_ServingCellInformation: Omit

maxAllowedUL_TX_Power:21

cellAccessRestriction:

cellBarred:

notBarred:

cellReservedForOperatorUse (ReservedIndicator):notReserved
cellReservationExtension (ReservedIndicator):notReserved

accessClassBarredList:

AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred
AccessClassBarred:notBarred

nonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]01 00 00 00 00 00 00 00
[8]00 00 00 00 00 00 11 00
[16]10 11 01 11 00 01 10 00
[24]00 00 00 00 00 01 00 00
[32]00 00 00 10 01 00 00 10
[40]00 00 01 00 01 11 11 11
[48]11 11 11 11 11 11 11 11

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:00:14.380

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:3

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:7
bcch_ModificationTime: Omit

#### PHY_DATA_REQ

MAC PHY @ 00:00:14.390

BTS unit: 1:2
Channel No: 0 Name: BCH
CFN: 168

Message Details:

SIB repetition period:64
SIB position:44
SIB size:246
SIB (raw):

[0]00 00 27 17 82 80 81 22
[8]F0 00 00 00 CB 71 80 01
[16]00 24 00 47 70 FF F8 01
[24]04 A1 4A 86 12 88 28 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 00 27 17 82 80 81 22
[8]F0 00 00 00 CB 71 80 01
[16]00 24 00 47 70 FF F8 01
[24]04 A1 4A 86 12 88 28

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:00:14.400

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:3

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:00:14.400

Channel ID: RbBcch
Cell ID: 3

Message Details:

RLC_TR_DATA_REQ:

cellId:3

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

completeSIB_List:

CompleteSIBshort:

sib_Type:systemInformationBlockType7
sib_Data_variable:100000101000000010000001

CompleteSIBshort:

sib_Type:systemInformationBlockType3
sib_Data_variable:0100000000000000000000000000110010110111000110000000000000010000000000100100001000000100011111111111111111111111

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:00:14.400

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 14

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

completeSIB_List:

CompleteSIB_List.element:

sib_Type: systemInformationBlockType7_SIB_Type [enum=7]

sib_Data_variable: 100000101000000010000001

CompleteSIB_List.element:

sib_Type: systemInformationBlockType3_SIB_Type [enum=3]

sib_Data_variable: 0100000000000000000000000000110010110111000110000000000000010000000000100100001000000100011111111111111111111111

Layer 3 SDU:

[0]00 0E 27 17 82 80 81 1B
[8]7A 00 00 00 65 B8 C0 00
[16]80 12 10 23 FF FF F8

#### o_SIB_PER_Encoding

RRC RRC @ 00:00:14.400

Category: TSO

Message Details:

Inputs:

SIB:

sIB18: (SysInfoType18)

idleModePLMNIdentities: (PLMNIdentitiesOfNeighbourCells)

plmnsOfIntraFreqCellsList: Omit

plmnsOfInterFreqCellsList: Omit

plmnsOfInterRATCellsList: Omit

connectedModePLMNIdentities: (PLMNIdentitiesOfNeighbourCells) Omit

nonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]10 00 00

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:00:14.400

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:3

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:23
bcch_ModificationTime: Omit

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:00:14.410

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:3

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:00:14.410

Channel ID: RbBcch
Cell ID: 3

Message Details:

RLC_TR_DATA_REQ:

cellId:3

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

completeSIB_List:

CompleteSIBshort:

sib_Type:systemInformationBlockType7
sib_Data_variable:100000101000000010000001

CompleteSIBshort:

sib_Type:systemInformationBlockType18
sib_Data_variable:100000

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:00:14.410

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 46

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

completeSIB_List:

CompleteSIB_List.element:

sib_Type: systemInformationBlockType7_SIB_Type [enum=7]

sib_Data_variable: 100000101000000010000001

CompleteSIB_List.element:

sib_Type: systemInformationBlockType18_SIB_Type [enum=26]

sib_Data_variable: 100000

Layer 3 SDU:

[0]00 0E 27 17 82 80 81 D0
[8]2C 00

#### o_SIB_PER_Encoding

RRC RRC @ 00:00:14.410

Category: TSO

Message Details:

Inputs:

SIB:

sIB4: (SysInfoType4)

cellIdentity:0000000000000000000000000011

cellSelectReselectInfo: (CellSelectReselectInfoSIB_3_4)

mappingInfo: Omit

cellSelectQualityMeasure:

cpich_RSCP:

modeSpecificInfo:

fdd:

s_Intrasearch (S_SearchQual):8
s_Intersearch (S_SearchQual):8
s_SearchHCS (S_SearchRXLEV): Omit

rat_List: (RAT_FDD_InfoList)

RAT_FDD_Info:

rat_Identifier:gsm
s_SearchRAT (S_SearchQual):-16
s_HCS_RAT (S_SearchRXLEV): Omit
s_Limit_SearchRAT (S_SearchQual):0

q_QualMin:-24
q_RxlevMin:-40

q_Hyst_l_S (Q_Hyst_S):0
t_Reselection_S:0

hcs_ServingCellInformation: Omit

maxAllowedUL_TX_Power:21

cellAccessRestriction:

cellBarred:

notBarred:

cellReservedForOperatorUse (ReservedIndicator):notReserved
cellReservationExtension (ReservedIndicator):notReserved

accessClassBarredList: Omit

nonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]00 00 00 00 00 00 00 00
[8]00 00 00 00 00 01 10 01
[16]01 10 11 10 00 11 00 00
[24]00 00 00 00 00 10 00 00
[32]00 00 01 00 10 00 00 00
[40]00 00 10 00 11 10 11 1

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:00:14.410

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:3

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:31
bcch_ModificationTime: Omit

#### PHY_DATA_REQ

MAC PHY @ 00:00:14.410

BTS unit: 1:2
Channel No: 0 Name: BCH
CFN: 170

Message Details:

SIB repetition period:64
SIB position:36
SIB size:246
SIB (raw):

[0]00 02 52 15 44 3E 00 FF
[8]43 FF FD D2 10 F0 29 0C
[16]0A A5 58 00 0C C5 B5 7E
[24]2B A0 FE 83 FA 0F E8 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 02 52 15 44 3E 00 FF
[8]43 FF FD D2 10 F0 29 0C
[16]0A A5 58 00 0C C5 B5 7E
[24]2B A0 FE 83 FA 0F E8

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:00:14.430

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:3

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:00:14.430

Channel ID: RbBcch
Cell ID: 3

Message Details:

RLC_TR_DATA_REQ:

cellId:3

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

completeSIB_List:

CompleteSIBshort:

sib_Type:systemInformationBlockType7
sib_Data_variable:100000101000000010000001

CompleteSIBshort:

sib_Type:systemInformationBlockType4
sib_Data_variable:00000000000000000000000000011001011011100011000000000000001000000000010010000000000010001110111

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:00:14.430

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 62

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

completeSIB_List:

CompleteSIB_List.element:

sib_Type: systemInformationBlockType7_SIB_Type [enum=7]

sib_Data_variable: 100000101000000010000001

CompleteSIB_List.element:

sib_Type: systemInformationBlockType4_SIB_Type [enum=4]

sib_Data_variable: 00000000000000000000000000011001011011100011000000000000001000000000010010000000000010001110111

Layer 3 SDU:

[0]00 0E 27 17 82 80 81 22
[8]F0 00 00 00 CB 71 80 01
[16]00 24 00 47 70

#### PHY_DATA_REQ

MAC PHY @ 00:00:14.430

BTS unit: 1:2
Channel No: 0 Name: BCH
CFN: 172

Message Details:

SIB repetition period:64
SIB position:38
SIB size:246
SIB (raw):

[0]00 04 50 0F F4 00 00 D6
[8]34 43 F4 E5 06 10 CA 03
[16]03 81 01 60 80 E0 08 86
[24]42 99 0A 00 30 11 14 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 04 50 0F F4 00 00 D6
[8]34 43 F4 E5 06 10 CA 03
[16]03 81 01 60 80 E0 08 86
[24]42 99 0A 00 30 11 14

#### o_SIB_PER_Encoding

RRC RRC @ 00:00:14.440

Category: TSO

Message Details:

Inputs:

SIB:

sIB11: (SysInfoType11)

sib12indicator:true

fach_MeasurementOccasionInfo: Omit

measurementControlSysInfo:

use_of_HCS:

hcs_not_used:

cellSelectQualityMeasure:

cpich_RSCP:

intraFreqMeasurementSysInfo: (IntraFreqMeasurementSysInfo_RSCP)

intraFreqMeasurementID (MeasurementIdentity): Omit

intraFreqCellInfoSI_List: (IntraFreqCellInfoSI_List_RSCP)

removedIntraFreqCellList: Omit

newIntraFreqCellList: (NewIntraFreqCellSI_List_RSCP)

NewIntraFreqCellSI_RSCP:

intraFreqCellID:3

cellInfo: (CellInfoSI_RSCP)

cellIndividualOffset: Omit

referenceTimeDifferenceToCell: Omit

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode:250

primaryCPICH_TX_Power: Omit
readSFN_Indicator:false
tx_DiversityIndicator:false

cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP) Omit

NewIntraFreqCellSI_RSCP:

intraFreqCellID:4

cellInfo: (CellInfoSI_RSCP)

cellIndividualOffset: Omit

referenceTimeDifferenceToCell: Omit

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode:300

primaryCPICH_TX_Power: Omit
readSFN_Indicator:true
tx_DiversityIndicator:false

cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP) Omit

NewIntraFreqCellSI_RSCP:

intraFreqCellID:5

cellInfo: (CellInfoSI_RSCP)

cellIndividualOffset: Omit

referenceTimeDifferenceToCell: Omit

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode:350

primaryCPICH_TX_Power: Omit
readSFN_Indicator:true
tx_DiversityIndicator:false

cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP) Omit

intraFreqMeasQuantity:

filterCoefficient: Omit

modeSpecificInfo:

fdd:

intraFreqMeasQuantity_FDD:cpich_RSCP

intraFreqReportingQuantityForRACH: Omit

maxReportedCellsOnRACH: Omit

reportingInfoForCellDCH:

intraFreqReportingQuantity:

activeSetReportingQuantities: (CellReportingQuantities)

dummy (SFN_SFN_OTD_Type):noReport
cellIdentity_reportingIndicator:true
cellSynchronisationInfoReportingIndicator:false

modeSpecificInfo:

fdd:

cpich_Ec_N0_reportingIndicator:false
cpich_RSCP_reportingIndicator:true
pathloss_reportingIndicator:false

monitoredSetReportingQuantities: (CellReportingQuantities)

dummy (SFN_SFN_OTD_Type):noReport
cellIdentity_reportingIndicator:true
cellSynchronisationInfoReportingIndicator:true

modeSpecificInfo:

fdd:

cpich_Ec_N0_reportingIndicator:false
cpich_RSCP_reportingIndicator:true
pathloss_reportingIndicator:false

detectedSetReportingQuantities: (CellReportingQuantities) Omit

measurementReportingMode:

measurementReportTransferMode (TransferMode):acknowledgedModeRLC
periodicalOrEventTrigger:eventTrigger

reportCriteria: (CellDCH_ReportCriteria)

intraFreqReportingCriteria:

eventCriteriaList: (IntraFreqEventCriteriaList)

IntraFreqEventCriteria:

event: (IntraFreqEvent)

e1a: (Event1a)

triggeringCondition (TriggeringCondition2):monitoredSetCellsOnly
reportingRange:5

forbiddenAffectCellList: Omit

w:1
reportDeactivationThreshold:t2
reportingAmount:ra4
reportingInterval:ri4

hysteresis:0
timeToTrigger:ttt640

reportingCellStatus:

withinActiveAndOrMonitoredUsedFreq (MaxNumberOfReportingCellsType1):e3

IntraFreqEventCriteria:

event: (IntraFreqEvent)

e1b: (Event1b)

triggeringCondition (TriggeringCondition1):activeSetCellsOnly
reportingRange:5

forbiddenAffectCellList: Omit

w:1

hysteresis:0
timeToTrigger:ttt640

reportingCellStatus:

withinActiveAndOrMonitoredUsedFreq (MaxNumberOfReportingCellsType1):e3

IntraFreqEventCriteria:

event: (IntraFreqEvent)

e1c: (Event1c)

replacementActivationThreshold:t3
reportingAmount:ra4
reportingInterval:ri4

hysteresis:0
timeToTrigger:ttt640

reportingCellStatus:

withinActiveAndOrMonitoredUsedFreq (MaxNumberOfReportingCellsType1):e3

interFreqMeasurementSysInfo: (InterFreqMeasurementSysInfo_RSCP)

interFreqCellInfoSI_List: (InterFreqCellInfoSI_List_RSCP)

removedInterFreqCellList: Omit

newInterFreqCellList: (NewInterFreqCellSI_List_RSCP)

NewInterFreqCellSI_RSCP:

interFreqCellID:0

frequencyInfo:

modeSpecificInfo:

fdd: (FrequencyInfoFDD)

uarfcn_UL (UARFCN): Omit
uarfcn_DL (UARFCN):10700

cellInfo: (CellInfoSI_RSCP)

cellIndividualOffset: Omit

referenceTimeDifferenceToCell: Omit

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode:100

primaryCPICH_TX_Power: Omit
readSFN_Indicator:false
tx_DiversityIndicator:false

cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP) Omit

NewInterFreqCellSI_RSCP:

interFreqCellID:1

frequencyInfo: Omit

cellInfo: (CellInfoSI_RSCP)

cellIndividualOffset: Omit

referenceTimeDifferenceToCell: Omit

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode:150

primaryCPICH_TX_Power: Omit
readSFN_Indicator:false
tx_DiversityIndicator:false

cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP) Omit

NewInterFreqCellSI_RSCP:

interFreqCellID:2

frequencyInfo: Omit

cellInfo: (CellInfoSI_RSCP)

cellIndividualOffset: Omit

referenceTimeDifferenceToCell: Omit

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode:200

primaryCPICH_TX_Power: Omit
readSFN_Indicator:false
tx_DiversityIndicator:false

cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP) Omit

NewInterFreqCellSI_RSCP:

interFreqCellID:6

frequencyInfo: Omit

cellInfo: (CellInfoSI_RSCP)

cellIndividualOffset: Omit

referenceTimeDifferenceToCell: Omit

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode:400

primaryCPICH_TX_Power: Omit
readSFN_Indicator:false
tx_DiversityIndicator:false

cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP) Omit

NewInterFreqCellSI_RSCP:

interFreqCellID:7

frequencyInfo: Omit

cellInfo: (CellInfoSI_RSCP)

cellIndividualOffset: Omit

referenceTimeDifferenceToCell: Omit

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode:450

primaryCPICH_TX_Power: Omit
readSFN_Indicator:false
tx_DiversityIndicator:false

cellSelectionReselectionInfo: (CellSelectReselectInfoSIB_11_12_RSCP) Omit

interRATMeasurementSysInfo: (InterRATMeasurementSysInfo_B) Omit

trafficVolumeMeasSysInfo: Omit

dummy: (UE_InternalMeasurementSysInfo) Omit

nonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]00 10 00 00 11 01 10 01
[8]00 00 10 10 00 11 00 00
[16]10 01 11 11 01 00 01 00
[24]10 00 00 01 01 00 10 11
[32]00 10 10 01 01 00 00 10
[40]10 10 11 11 01 00 00 10
[48]00 10 00 10 00 11 00 10
[56]01 01 01 01 00 00 00 01
[64]00 10 10 00 01 01 00 10
[72]10 10 00 01 10 00 01 00
[80]10 10 00 10 00 00 10 10
[88]00 01 00 00 11 00 00 10
[96]01 01 00 10 01 10 10 10
[104]10 00 01 10 00 01 00 10
[112]10 10 01 00 11 00 00 00
[120]01 01 00 11 10 01 10 00
[128]00 01 00 01 10 01 00 00
[136]10 00 00 10 00 01 00 10
[144]01 01 10 00 10 00 01 00
[152]00 01 00 11 00 10 00 00
[160]10 00 11 00 00 01 01 10
[168]01 00 00 00 10 00 11 10
[176]00 01 01 11 00 00 10 00

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:00:14.440

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:3

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:30
bcch_ModificationTime: Omit

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:00:14.460

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:3

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:00:14.460

Channel ID: RbBcch
Cell ID: 3

Message Details:

RLC_TR_DATA_REQ:

cellId:3

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

noSegment:

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:00:14.460

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 60

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

noSegment: NULL

Layer 3 SDU:

[0]00 00

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:00:14.460

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:3

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:29
bcch_ModificationTime: Omit

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:00:14.470

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:3

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:00:14.470

Channel ID: RbBcch
Cell ID: 3

Message Details:

RLC_TR_DATA_REQ:

cellId:3

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

noSegment:

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:00:14.470

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 58

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

noSegment: NULL

Layer 3 SDU:

[0]00 00

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:00:14.470

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:3

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:26
bcch_ModificationTime: Omit

#### MAC_DATA_REQ

RLC MAC @ 00:00:14.470

Category: Configuration
BTS unit: 1:2
Channel No: 0 Name: BCCH
CFN: 176

Message Details:

RLC PDU size (bits):168
RLC PDU (raw):

[0]00 06 51 81 CA D6 80 07
[8]88 60 16 DB 62 00 43 08
[16]94 0B 68 04 00

#### MAC_DATA_REQ

RLC MAC @ 00:00:14.470

Category: Configuration
BTS unit: 1:2
Channel No: 0 Name: BCCH
CFN: 176

Message Details:

RLC PDU size (bits):48
RLC PDU (raw):

[0]00 0E 06 0F 02 91

#### MAC_DATA_REQ

RLC MAC @ 00:00:14.470

Category: Configuration
BTS unit: 1:2
Channel No: 0 Name: BCCH
CFN: 176

Message Details:

RLC PDU size (bits):16
RLC PDU (raw):

[0]00 00

#### MAC_DATA_REQ

RLC MAC @ 00:00:14.470

Category: Configuration
BTS unit: 1:2
Channel No: 0 Name: BCCH
CFN: 176

Message Details:

RLC PDU size (bits):16
RLC PDU (raw):

[0]00 00

#### MAC_DATA_REQ

RLC MAC @ 00:00:14.470

Category: Configuration
BTS unit: 1:2
Channel No: 0 Name: BCCH
CFN: 176

Message Details:

RLC PDU size (bits):16
RLC PDU (raw):

[0]00 00

#### MAC_DATA_REQ

RLC MAC @ 00:00:14.470

Category: Configuration
BTS unit: 1:2
Channel No: 0 Name: BCCH
CFN: 176

Message Details:

RLC PDU size (bits):56
RLC PDU (raw):

[0]00 0E 07 17 82 80 81

#### MAC_DATA_REQ

RLC MAC @ 00:00:14.470

Category: Configuration
BTS unit: 1:2
Channel No: 0 Name: BCCH
CFN: 176

Message Details:

RLC PDU size (bits):184
RLC PDU (raw):

[0]00 0E 27 17 82 80 81 1B
[8]7A 00 00 00 65 B8 C0 00
[16]80 12 10 23 FF FF F8

#### MAC_DATA_REQ

RLC MAC @ 00:00:14.470

Category: Configuration
BTS unit: 1:2
Channel No: 0 Name: BCCH
CFN: 176

Message Details:

RLC PDU size (bits):80
RLC PDU (raw):

[0]00 0E 27 17 82 80 81 D0
[8]2C 00

#### MAC_DATA_REQ

RLC MAC @ 00:00:14.470

Category: Configuration
BTS unit: 1:2
Channel No: 0 Name: BCCH
CFN: 176

Message Details:

RLC PDU size (bits):168
RLC PDU (raw):

[0]00 0E 27 17 82 80 81 22
[8]F0 00 00 00 CB 71 80 01
[16]00 24 00 47 70

#### PHY_DATA_REQ

MAC PHY @ 00:00:14.470

BTS unit: 1:2
Channel No: 0 Name: BCH
CFN: 176

Message Details:

SIB repetition period:64
SIB position:42
SIB size:246
SIB (raw):

[0]00 06 51 81 CA D6 80 07
[8]88 60 16 DB 62 00 43 08
[16]94 0B 68 04 00 E0 08 86
[24]42 99 0A 00 30 11 14 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 06 51 81 CA D6 80 07
[8]88 60 16 DB 62 00 43 08
[16]94 0B 68 04 00 E0 08 86
[24]42 99 0A 00 30 11 14

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:00:14.490

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:3

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:00:14.490

Channel ID: RbBcch
Cell ID: 3

Message Details:

RLC_TR_DATA_REQ:

cellId:3

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

firstSegment:

sib_Type:systemInformationBlockType11
seg_Count (SegCount):2
sib_Data_fixed:001000001101100100001010001100001001111101000100100000010100101100101001010000101010111101000010001000100011001001010101000000010010100001010010101000011000010010100010000010100001000011000010010100100110101010000110000100

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:00:14.490

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 52

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

firstSegment:

sib_Type: systemInformationBlockType11_SIB_Type [enum=11]

seg_Count: 2

sib_Data_fixed: 001000001101100100001010001100001001111101000100100000010100101100101001010000101010111101000010001000100011001001010101000000010010100001010010101000011000010010100010000010100001000011000010010100100110101010000110000100

Layer 3 SDU:

[0]00 02 B1 20 D9 0A 30 9F
[8]44 81 4B 29 42 AF 42 22
[16]32 55 01 28 52 A1 84 A2
[24]0A 10 C2 52 6A 86 10

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:00:14.490

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:3

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:27
bcch_ModificationTime: Omit

#### PHY_DATA_REQ

MAC PHY @ 00:00:14.490

BTS unit: 1:2
Channel No: 0 Name: BCH
CFN: 178

Message Details:

SIB repetition period:64
SIB position:4
SIB size:246
SIB (raw):

[0]00 0E 06 0F 02 91 80 07
[8]88 60 16 DB 62 00 43 08
[16]94 0B 68 04 00 E0 08 86
[24]42 99 0A 00 30 11 14 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 0E 06 0F 02 91 80 07
[8]88 60 16 DB 62 00 43 08
[16]94 0B 68 04 00 E0 08 86
[24]42 99 0A 00 30 11 14

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:00:14.500

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:3

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:00:14.500

Channel ID: RbBcch
Cell ID: 3

Message Details:

RLC_TR_DATA_REQ:

cellId:3

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

lastSegmentShort:

sib_Type:systemInformationBlockType11
segmentIndex:1
sib_Data_variable:10101001001100000001010011100110000001000110010000100000100001001001011000100001000001001100100000100011000001011001000000100011100001011100001000

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:00:14.500

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 54

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

lastSegmentShort:

sib_Type: systemInformationBlockType11_SIB_Type [enum=11]

segmentIndex: 1

sib_Data_variable: 10101001001100000001010011100110000001000110010000100000100001001001011000100001000001001100100000100011000001011001000000100011100001011100001000

Layer 3 SDU:

[0]00 06 B0 91 A9 30 14 E6
[8]04 64 20 84 96 21 04 C8
[16]23 05 90 23 85 C2 00

#### o_SIB_PER_Encoding

RRC RRC @ 00:00:14.500

Category: TSO

Message Details:

Inputs:

SIB:

sIB12: (SysInfoType12)

fach_MeasurementOccasionInfo: Omit

measurementControlSysInfo:

use_of_HCS:

hcs_not_used:

cellSelectQualityMeasure:

cpich_RSCP:

intraFreqMeasurementSysInfo: (IntraFreqMeasurementSysInfo_RSCP) Omit

interFreqMeasurementSysInfo: (InterFreqMeasurementSysInfo_RSCP) Omit

interRATMeasurementSysInfo: (InterRATMeasurementSysInfo_B) Omit

trafficVolumeMeasSysInfo: Omit

dummy: (UE_InternalMeasurementSysInfo) Omit

nonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]00 00 00 00 0

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:00:14.500

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:3

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:11
bcch_ModificationTime: Omit

#### PHY_DATA_REQ

MAC PHY @ 00:00:14.510

BTS unit: 1:2
Channel No: 0 Name: BCH
CFN: 180

Message Details:

SIB repetition period:64
SIB position:6
SIB size:246
SIB (raw):

[0]00 00 06 0F 02 91 80 07
[8]88 60 16 DB 62 00 43 08
[16]94 0B 68 04 00 E0 08 86
[24]42 99 0A 00 30 11 14 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 00 06 0F 02 91 80 07
[8]88 60 16 DB 62 00 43 08
[16]94 0B 68 04 00 E0 08 86
[24]42 99 0A 00 30 11 14

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:00:14.520

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:3

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:00:14.520

Channel ID: RbBcch
Cell ID: 3

Message Details:

RLC_TR_DATA_REQ:

cellId:3

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

completeSIB_List:

CompleteSIBshort:

sib_Type:systemInformationBlockType12
sib_Data_variable:000000000

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:00:14.520

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 22

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

completeSIB_List:

CompleteSIB_List.element:

sib_Type: systemInformationBlockType12_SIB_Type [enum=12]

sib_Data_variable: 000000000

Layer 3 SDU:

[0]00 0E 0C 08 00 00

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:00:14.520

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:3

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:13
bcch_ModificationTime: Omit

#### MAC_DATA_REQ

RLC MAC @ 00:00:14.520

Category: Configuration
BTS unit: 1:2
Channel No: 0 Name: BCCH
CFN: 181

Message Details:

RLC PDU size (bits):16
RLC PDU (raw):

[0]00 00

#### MAC_DATA_REQ

RLC MAC @ 00:00:14.520

Category: Configuration
BTS unit: 1:2
Channel No: 0 Name: BCCH
CFN: 181

Message Details:

RLC PDU size (bits):16
RLC PDU (raw):

[0]00 00

#### MAC_DATA_REQ

RLC MAC @ 00:00:14.520

Category: Configuration
BTS unit: 1:2
Channel No: 0 Name: BCCH
CFN: 181

Message Details:

RLC PDU size (bits):248
RLC PDU (raw):

[0]00 02 B1 20 D9 0A 30 9F
[8]44 81 4B 29 42 AF 42 22
[16]32 55 01 28 52 A1 84 A2
[24]0A 10 C2 52 6A 86 10

#### PHY_DATA_REQ

MAC PHY @ 00:00:14.530

BTS unit: 1:2
Channel No: 0 Name: BCH
CFN: 182

Message Details:

SIB repetition period:64
SIB position:10
SIB size:246
SIB (raw):

[0]00 00 06 0F 02 91 80 07
[8]88 60 16 DB 62 00 43 08
[16]94 0B 68 04 00 E0 08 86
[24]42 99 0A 00 30 11 14 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 00 06 0F 02 91 80 07
[8]88 60 16 DB 62 00 43 08
[16]94 0B 68 04 00 E0 08 86
[24]42 99 0A 00 30 11 14

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:00:14.540

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:3

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:00:14.540

Channel ID: RbBcch
Cell ID: 3

Message Details:

RLC_TR_DATA_REQ:

cellId:3

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

noSegment:

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:00:14.540

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 26

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

noSegment: NULL

Layer 3 SDU:

[0]00 00

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:00:14.540

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:3

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:14
bcch_ModificationTime: Omit

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:00:14.550

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:3

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:00:14.550

Channel ID: RbBcch
Cell ID: 3

Message Details:

RLC_TR_DATA_REQ:

cellId:3

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

noSegment:

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:00:14.550

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 28

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

noSegment: NULL

Layer 3 SDU:

[0]00 00

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:00:14.550

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:3

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:15
bcch_ModificationTime: Omit

#### PHY_DATA_REQ

MAC PHY @ 00:00:14.550

BTS unit: 1:2
Channel No: 0 Name: BCH
CFN: 184

Message Details:

SIB repetition period:64
SIB position:12
SIB size:246
SIB (raw):

[0]00 00 06 0F 02 91 80 07
[8]88 60 16 DB 62 00 43 08
[16]94 0B 68 04 00 E0 08 86
[24]42 99 0A 00 30 11 14 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 00 06 0F 02 91 80 07
[8]88 60 16 DB 62 00 43 08
[16]94 0B 68 04 00 E0 08 86
[24]42 99 0A 00 30 11 14

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:00:14.570

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:3

routingInfo:

rB_Identity:-1

#### o_SIB_PER_Encoding

RRC RRC @ 00:00:14.570

Category: TSO

Message Details:

Inputs:

SIB:

sIB7: (SysInfoType7)

modeSpecificInfo:

fdd:

ul_Interference:-100

prach_Information_SIB5_List: (DynamicPersistenceLevelList)

DynamicPersistenceLevel:2

prach_Information_SIB6_List: (DynamicPersistenceLevelList)

DynamicPersistenceLevel:2

expirationTimeFactor: Omit

nonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]10 00 00 10 10 00 00 00
[8]10 00 00 01

#### RLC_TR_DATA_REQ

RRC LLA @ 00:00:14.570

Channel ID: RbBcch
Cell ID: 3

Message Details:

RLC_TR_DATA_REQ:

cellId:3

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

completeSIB_List:

CompleteSIBshort:

sib_Type:systemInformationBlockType7
sib_Data_variable:100000101000000010000001

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:00:14.570

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 30

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

completeSIB_List:

CompleteSIB_List.element:

sib_Type: systemInformationBlockType7_SIB_Type [enum=7]

sib_Data_variable: 100000101000000010000001

Layer 3 SDU:

[0]00 0E 07 17 82 80 81

#### o_SIB_PER_Encoding

RRC RRC @ 00:00:14.570

Category: TSO

Message Details:

Inputs:

SIB:

sIB18: (SysInfoType18)

idleModePLMNIdentities: (PLMNIdentitiesOfNeighbourCells)

plmnsOfIntraFreqCellsList: Omit

plmnsOfInterFreqCellsList: Omit

plmnsOfInterRATCellsList: Omit

connectedModePLMNIdentities: (PLMNIdentitiesOfNeighbourCells) Omit

nonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]10 00 00

#### o_SIB_PER_Encoding

RRC RRC @ 00:00:14.570

Category: TSO

Message Details:

Inputs:

SIB:

sIB7: (SysInfoType7)

modeSpecificInfo:

fdd:

ul_Interference:-100

prach_Information_SIB5_List: (DynamicPersistenceLevelList)

DynamicPersistenceLevel:2

prach_Information_SIB6_List: (DynamicPersistenceLevelList)

DynamicPersistenceLevel:2

expirationTimeFactor: Omit

nonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]10 00 00 10 10 00 00 00
[8]10 00 00 01

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:00:14.570

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:3

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:6
sg_POS:23
bcch_ModificationTime: Omit

#### PHY_DATA_REQ

MAC PHY @ 00:00:14.570

BTS unit: 1:2
Channel No: 0 Name: BCH
CFN: 186

Message Details:

SIB repetition period:64
SIB position:30
SIB size:246
SIB (raw):

[0]00 0E 07 17 82 80 81 07
[8]88 60 16 DB 62 00 43 08
[16]94 0B 68 04 00 E0 08 86
[24]42 99 0A 00 30 11 14 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 0E 07 17 82 80 81 07
[8]88 60 16 DB 62 00 43 08
[16]94 0B 68 04 00 E0 08 86
[24]42 99 0A 00 30 11 14

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:00:14.580

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:3

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:00:14.580

Channel ID: RbBcch
Cell ID: 3

Message Details:

RLC_TR_DATA_REQ:

cellId:3

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

completeSIB_List:

CompleteSIBshort:

sib_Type:systemInformationBlockType7
sib_Data_variable:100000101000000010000001

CompleteSIBshort:

sib_Type:systemInformationBlockType18
sib_Data_variable:100000

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:00:14.580

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 64

SIB position: 46

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

completeSIB_List:

CompleteSIB_List.element:

sib_Type: systemInformationBlockType7_SIB_Type [enum=7]

sib_Data_variable: 100000101000000010000001

CompleteSIB_List.element:

sib_Type: systemInformationBlockType18_SIB_Type [enum=26]

sib_Data_variable: 100000

Layer 3 SDU:

[0]00 0E 27 17 82 80 81 D0
[8]2C 00

#### o_SIB_PER_Encoding

RRC RRC @ 00:00:14.580

Category: TSO

Message Details:

Inputs:

SIB:

sB1: (SysInfoTypeSB1)

sib_ReferenceList:

SchedulingInformationSIB:

sib_Type: (SIB_TypeAndTag)

sysInfoType6 (CellValueTag):2

scheduling: (SchedulingInformation)

scheduling:

segCount: Omit

sib_Pos:

rep64:2

sib_PosOffsetInfo: (SibOFF_List) Omit

SchedulingInformationSIB:

sib_Type: (SIB_TypeAndTag)

sysInfoType7:

scheduling: (SchedulingInformation)

scheduling:

segCount: Omit

sib_Pos:

rep16:7

sib_PosOffsetInfo: (SibOFF_List) Omit

SchedulingInformationSIB:

sib_Type: (SIB_TypeAndTag)

sysInfoType11 (CellValueTag):2

scheduling: (SchedulingInformation)

scheduling:

segCount:2

sib_Pos:

rep64:26

sib_PosOffsetInfo: (SibOFF_List)

SibOFF:so2

SchedulingInformationSIB:

sib_Type: (SIB_TypeAndTag)

sysInfoType12 (CellValueTag):2

scheduling: (SchedulingInformation)

scheduling:

segCount: Omit

sib_Pos:

rep64:11

sib_PosOffsetInfo: (SibOFF_List) Omit

SchedulingInformationSIB:

sib_Type: (SIB_TypeAndTag)

sysInfoType18 (CellValueTag):2

scheduling: (SchedulingInformation)

scheduling:

segCount: Omit

sib_Pos:

rep64:23

sib_PosOffsetInfo: (SibOFF_List) Omit

nonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]00 01 00 00 10 10 10 00
[8]10 00 00 10 00 11 00 00
[16]01 01 11 01 01 00 11 10
[24]00 10 10 01 10 10 00 00
[32]00 00 01 01 10 10 00 10
[40]00 10 11 11 00 10 10 00
[48]10 01 01 11

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:00:14.580

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:3

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:4
sg_POS:1
bcch_ModificationTime: Omit

#### PHY_DATA_REQ

MAC PHY @ 00:00:14.590

BTS unit: 1:2
Channel No: 0 Name: BCH
CFN: 188

Message Details:

SIB repetition period:64
SIB position:14
SIB size:246
SIB (raw):

[0]00 0E 27 17 82 80 81 1B
[8]7A 00 00 00 65 B8 C0 00
[16]80 12 10 23 FF FF F8 86
[24]42 99 0A 00 30 11 14 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 0E 27 17 82 80 81 1B
[8]7A 00 00 00 65 B8 C0 00
[16]80 12 10 23 FF FF F8 86
[24]42 99 0A 00 30 11 14

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:00:14.600

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:3

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:00:14.600

Channel ID: RbBcch
Cell ID: 3

Message Details:

RLC_TR_DATA_REQ:

cellId:3

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

completeSIB_List:

CompleteSIBshort:

sib_Type:schedulingBlock1
sib_Data_variable:00010000101010001000001000110000010111010100111000101001101000000000010110100010001011110010100010010111

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:00:14.600

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 16

SIB position: 2

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

completeSIB_List:

CompleteSIB_List.element:

sib_Type: schedulingBlock1_SIB_Type [enum=27]

sib_Data_variable: 00010000101010001000001000110000010111010100111000101001101000000000010110100010001011110010100010010111

Layer 3 SDU:

[0]00 0E 1B 67 10 A8 82 30
[8]5D 4E 29 A0 05 A2 2F 28
[16]97

#### o_SIB_PER_Encoding

RRC RRC @ 00:00:14.600

Category: TSO

Message Details:

Inputs:

SIB:

mIB: (MasterInformationBlock)

mib_ValueTag:2

plmn_Type:

gsm_MAP:

plmn_Identity:

mcc:

Digit:0
Digit:0
Digit:1

mnc:

Digit:0
Digit:1

sibSb_ReferenceList:

SchedulingInformationSIBSb:

sibSb_Type: (SIBSb_TypeAndTag)

sysInfoTypeSB1 (CellValueTag):2

scheduling: (SchedulingInformation)

scheduling:

segCount: Omit

sib_Pos:

rep16:1

sib_PosOffsetInfo: (SibOFF_List) Omit

SchedulingInformationSIBSb:

sibSb_Type: (SIBSb_TypeAndTag)

sysInfoType1 (PLMN_ValueTag):2

scheduling: (SchedulingInformation)

scheduling:

segCount: Omit

sib_Pos:

rep64:10

sib_PosOffsetInfo: (SibOFF_List) Omit

SchedulingInformationSIBSb:

sibSb_Type: (SIBSb_TypeAndTag)

sysInfoType2 (CellValueTag):2

scheduling: (SchedulingInformation)

scheduling:

segCount: Omit

sib_Pos:

rep64:10

sib_PosOffsetInfo: (SibOFF_List) Omit

SchedulingInformationSIBSb:

sibSb_Type: (SIBSb_TypeAndTag)

sysInfoType3 (CellValueTag):2

scheduling: (SchedulingInformation)

scheduling:

segCount: Omit

sib_Pos:

rep64:7

sib_PosOffsetInfo: (SibOFF_List) Omit

SchedulingInformationSIBSb:

sibSb_Type: (SIBSb_TypeAndTag)

sysInfoType4 (CellValueTag):2

scheduling: (SchedulingInformation)

scheduling:

segCount: Omit

sib_Pos:

rep64:31

sib_PosOffsetInfo: (SibOFF_List) Omit

SchedulingInformationSIBSb:

sibSb_Type: (SIBSb_TypeAndTag)

sysInfoType5 (CellValueTag):2

scheduling: (SchedulingInformation)

scheduling:

segCount:3

sib_Pos:

rep64:18

sib_PosOffsetInfo: (SibOFF_List)

SibOFF:so2
SibOFF:so4

nonCriticalExtensions: Omit

Outputs:

BITSTRING:

[0]00 01 00 00 00 00 00 00
[8]01 00 00 00 00 10 01 01
[16]10 10 10 10 00 01 00 01
[24]00 00 00 00 00 00 10 00
[32]10 00 10 10 00 00 10 10
[40]00 10 00 10 10 00 01 00
[48]10 00 10 00 01 11 00 01
[56]10 10 00 10 01 11 11 00
[64]10 00 11 10 01 00 10 01
[72]00 10 00 01 00 00 00 01

#### CMAC_SYSINFO_Config_REQ

RRC LLA @ 00:00:14.600

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_REQ:

cellId:3

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CmacSysinfoConfigReq)

sg_REP:3
sg_POS:0
bcch_ModificationTime: Omit

#### CMAC_SYSINFO_Config_CNF

LLA RRC @ 00:00:14.610

Channel ID: RbBcch
Cell ID: 3

Message Details:

CMAC_SYSINFO_Config_CNF:

cellId:3

routingInfo:

rB_Identity:-1

#### RLC_TR_DATA_REQ

RRC LLA @ 00:00:14.610

Channel ID: RbBcch
Cell ID: 3

Message Details:

RLC_TR_DATA_REQ:

cellId:3

routingInfo:

rB_Identity:-1

tM_message:

bCCH_BCH_Message:

message: (SystemInformation_BCH)

sfn_Prime:0

payload:

completeSIB_List:

CompleteSIBshort:

sib_Type:masterInformationBlock
sib_Data_variable:0001000000000000010000000010010110101010000100010000000000001000100010100000101000100010100001001000100001110001101000100111110010001110010010010010000100000001

#### RLC_TR_DATA_REQ: SystemInformation-BCH

LLA RLC @ 00:00:14.610

Channel No: 0 Name: BCCH

Message Details:

SIB repetition rate: 8

SIB position: 0

BCCH_BCH_Message:

message:

sfn_Prime: 0

payload:

completeSIB_List:

CompleteSIB_List.element:

sib_Type: masterInformationBlock_SIB_Type [enum=0]

sib_Data_variable: 0001000000000000010000000010010110101010000100010000000000001000100010100000101000100010100001001000100001110001101000100111110010001110010010010010000100000001

Layer 3 SDU:

[0]00 0E 00 9F 10 00 40 25
[8]AA 11 00 08 8A 0A 22 84
[16]88 71 A2 7C 8E 49 21 01

#### MMI_CmdReq

RRC LLA @ 00:00:14.610

Message Details:

MMI_CmdReq:

cmd (IA5String):Please switch on the UE

#### PHY_DATA_REQ

MAC PHY @ 00:00:14.610

BTS unit: 1:2
Channel No: 0 Name: BCH
CFN: 190

Message Details:

SIB repetition period:64
SIB position:46
SIB size:246
SIB (raw):

[0]00 0E 27 17 82 80 81 D0
[8]2C 00 00 00 65 B8 C0 00
[16]80 12 10 23 FF FF F8 86
[24]42 99 0A 00 30 11 14 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 0E 27 17 82 80 81 D0
[8]2C 00 00 00 65 B8 C0 00
[16]80 12 10 23 FF FF F8 86
[24]42 99 0A 00 30 11 14

#### MAC_DATA_REQ

RLC MAC @ 00:00:14.630

Category: Configuration
BTS unit: 1:2
Channel No: 0 Name: BCCH
CFN: 192

Message Details:

RLC PDU size (bits):184
RLC PDU (raw):

[0]00 06 B0 91 A9 30 14 E6
[8]04 64 20 84 96 21 04 C8
[16]23 05 90 23 85 C2 00

#### MAC_DATA_REQ

RLC MAC @ 00:00:14.630

Category: Configuration
BTS unit: 1:2
Channel No: 0 Name: BCCH
CFN: 192

Message Details:

RLC PDU size (bits):48
RLC PDU (raw):

[0]00 0E 0C 08 00 00

#### MAC_DATA_REQ

RLC MAC @ 00:00:14.630

Category: Configuration
BTS unit: 1:2
Channel No: 0 Name: BCCH
CFN: 192

Message Details:

RLC PDU size (bits):16
RLC PDU (raw):

[0]00 00

#### MAC_DATA_REQ

RLC MAC @ 00:00:14.630

Category: Configuration
BTS unit: 1:2
Channel No: 0 Name: BCCH
CFN: 192

Message Details:

RLC PDU size (bits):16
RLC PDU (raw):

[0]00 00

#### MAC_DATA_REQ

RLC MAC @ 00:00:14.630

Category: Configuration
BTS unit: 1:2
Channel No: 0 Name: BCCH
CFN: 192

Message Details:

RLC PDU size (bits):56
RLC PDU (raw):

[0]00 0E 07 17 82 80 81

#### MAC_DATA_REQ

RLC MAC @ 00:00:14.630

Category: Configuration
BTS unit: 1:2
Channel No: 0 Name: BCCH
CFN: 192

Message Details:

RLC PDU size (bits):80
RLC PDU (raw):

[0]00 0E 27 17 82 80 81 D0
[8]2C 00

#### MAC_DATA_REQ

RLC MAC @ 00:00:14.630

Category: Configuration
BTS unit: 1:2
Channel No: 0 Name: BCCH
CFN: 192

Message Details:

RLC PDU size (bits):136
RLC PDU (raw):

[0]00 0E 1B 67 10 A8 82 30
[8]5D 4E 29 A0 05 A2 2F 28
[16]97

#### PHY_DATA_REQ

MAC PHY @ 00:00:14.630

BTS unit: 1:2
Channel No: 0 Name: BCH
CFN: 192

Message Details:

SIB repetition period:64
SIB position:62
SIB size:246
SIB (raw):

[0]00 0E 27 17 82 80 81 22
[8]F0 00 00 00 CB 71 80 01
[16]00 24 00 47 70 FF F8 86
[24]42 99 0A 00 30 11 14 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 0E 27 17 82 80 81 22
[8]F0 00 00 00 CB 71 80 01
[16]00 24 00 47 70 FF F8 86
[24]42 99 0A 00 30 11 14

#### PHY_DATA_REQ

MAC PHY @ 00:00:14.650

BTS unit: 1:2
Channel No: 0 Name: BCH
CFN: 194

Message Details:

SIB repetition period:64
SIB position:60
SIB size:246
SIB (raw):

[0]00 00 27 17 82 80 81 22
[8]F0 00 00 00 CB 71 80 01
[16]00 24 00 47 70 FF F8 86
[24]42 99 0A 00 30 11 14 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 00 27 17 82 80 81 22
[8]F0 00 00 00 CB 71 80 01
[16]00 24 00 47 70 FF F8 86
[24]42 99 0A 00 30 11 14

#### PHY_DATA_REQ

MAC PHY @ 00:00:14.670

BTS unit: 1:2
Channel No: 0 Name: BCH
CFN: 196

Message Details:

SIB repetition period:64
SIB position:58
SIB size:246
SIB (raw):

[0]00 00 27 17 82 80 81 22
[8]F0 00 00 00 CB 71 80 01
[16]00 24 00 47 70 FF F8 86
[24]42 99 0A 00 30 11 14 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 00 27 17 82 80 81 22
[8]F0 00 00 00 CB 71 80 01
[16]00 24 00 47 70 FF F8 86
[24]42 99 0A 00 30 11 14

#### PHY_DATA_REQ

MAC PHY @ 00:00:14.690

BTS unit: 1:2
Channel No: 0 Name: BCH
CFN: 198

Message Details:

SIB repetition period:64
SIB position:52
SIB size:246
SIB (raw):

[0]00 02 B1 20 D9 0A 30 9F
[8]44 81 4B 29 42 AF 42 22
[16]32 55 01 28 52 A1 84 A2
[24]0A 10 C2 52 6A 86 10 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 02 B1 20 D9 0A 30 9F
[8]44 81 4B 29 42 AF 42 22
[16]32 55 01 28 52 A1 84 A2
[24]0A 10 C2 52 6A 86 10

#### PHY_DATA_REQ

MAC PHY @ 00:00:14.710

BTS unit: 1:2
Channel No: 0 Name: BCH
CFN: 200

Message Details:

SIB repetition period:64
SIB position:54
SIB size:246
SIB (raw):

[0]00 06 B0 91 A9 30 14 E6
[8]04 64 20 84 96 21 04 C8
[16]23 05 90 23 85 C2 00 A2
[24]0A 10 C2 52 6A 86 10 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 06 B0 91 A9 30 14 E6
[8]04 64 20 84 96 21 04 C8
[16]23 05 90 23 85 C2 00 A2
[24]0A 10 C2 52 6A 86 10

#### MAC_DATA_REQ

RLC MAC @ 00:00:14.730

Category: Configuration
BTS unit: 1:2
Channel No: 0 Name: BCCH
CFN: 202

Message Details:

RLC PDU size (bits):192
RLC PDU (raw):

[0]00 0E 00 9F 10 00 40 25
[8]AA 11 00 08 8A 0A 22 84
[16]88 71 A2 7C 8E 49 21 01

#### PHY_DATA_REQ

MAC PHY @ 00:00:14.730

BTS unit: 1:2
Channel No: 0 Name: BCH
CFN: 202

Message Details:

SIB repetition period:64
SIB position:22
SIB size:246
SIB (raw):

[0]00 0E 0C 08 00 00 14 E6
[8]04 64 20 84 96 21 04 C8
[16]23 05 90 23 85 C2 00 A2
[24]0A 10 C2 52 6A 86 10 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 0E 0C 08 00 00 14 E6
[8]04 64 20 84 96 21 04 C8
[16]23 05 90 23 85 C2 00 A2
[24]0A 10 C2 52 6A 86 10

#### PHY_DATA_REQ

MAC PHY @ 00:00:14.750

BTS unit: 1:2
Channel No: 0 Name: BCH
CFN: 204

Message Details:

SIB repetition period:64
SIB position:26
SIB size:246
SIB (raw):

[0]00 00 0C 08 00 00 14 E6
[8]04 64 20 84 96 21 04 C8
[16]23 05 90 23 85 C2 00 A2
[24]0A 10 C2 52 6A 86 10 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 00 0C 08 00 00 14 E6
[8]04 64 20 84 96 21 04 C8
[16]23 05 90 23 85 C2 00 A2
[24]0A 10 C2 52 6A 86 10

#### PHY_DATA_REQ

MAC PHY @ 00:00:14.770

BTS unit: 1:2
Channel No: 0 Name: BCH
CFN: 206

Message Details:

SIB repetition period:64
SIB position:28
SIB size:246
SIB (raw):

[0]00 00 0C 08 00 00 14 E6
[8]04 64 20 84 96 21 04 C8
[16]23 05 90 23 85 C2 00 A2
[24]0A 10 C2 52 6A 86 10 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 00 0C 08 00 00 14 E6
[8]04 64 20 84 96 21 04 C8
[16]23 05 90 23 85 C2 00 A2
[24]0A 10 C2 52 6A 86 10

#### PHY_DATA_REQ

MAC PHY @ 00:00:14.790

BTS unit: 1:2
Channel No: 0 Name: BCH
CFN: 208

Message Details:

SIB repetition period:64
SIB position:30
SIB size:246
SIB (raw):

[0]00 0E 07 17 82 80 81 E6
[8]04 64 20 84 96 21 04 C8
[16]23 05 90 23 85 C2 00 A2
[24]0A 10 C2 52 6A 86 10 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 0E 07 17 82 80 81 E6
[8]04 64 20 84 96 21 04 C8
[16]23 05 90 23 85 C2 00 A2
[24]0A 10 C2 52 6A 86 10

#### PHY_DATA_REQ

MAC PHY @ 00:00:14.810

BTS unit: 1:2
Channel No: 0 Name: BCH
CFN: 210

Message Details:

SIB repetition period:64
SIB position:46
SIB size:246
SIB (raw):

[0]00 0E 27 17 82 80 81 D0
[8]2C 00 20 84 96 21 04 C8
[16]23 05 90 23 85 C2 00 A2
[24]0A 10 C2 52 6A 86 10 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 0E 27 17 82 80 81 D0
[8]2C 00 20 84 96 21 04 C8
[16]23 05 90 23 85 C2 00 A2
[24]0A 10 C2 52 6A 86 10

#### PHY_DATA_REQ

MAC PHY @ 00:00:14.830

BTS unit: 1:2
Channel No: 0 Name: BCH
CFN: 212

Message Details:

SIB repetition period:16
SIB position:2
SIB size:246
SIB (raw):

[0]00 0E 1B 67 10 A8 82 30
[8]5D 4E 29 A0 05 A2 2F 28
[16]97 05 90 23 85 C2 00 A2
[24]0A 10 C2 52 6A 86 10 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 0E 1B 67 10 A8 82 30
[8]5D 4E 29 A0 05 A2 2F 28
[16]97 05 90 23 85 C2 00 A2
[24]0A 10 C2 52 6A 86 10

#### PHY_DATA_REQ

MAC PHY @ 00:00:14.850

BTS unit: 1:2
Channel No: 0 Name: BCH
CFN: 214

Message Details:

SIB repetition period:8
SIB position:0
SIB size:246
SIB (raw):

[0]00 0E 00 9F 10 00 40 25
[8]AA 11 00 08 8A 0A 22 84
[16]88 71 A2 7C 8E 49 21 01
[24]0A 10 C2 52 6A 86 10 00

SIB (decoded):

TB 0:

MAC SDU (246 bits):

[0]00 0E 00 9F 10 00 40 25
[8]AA 11 00 08 8A 0A 22 84
[16]88 71 A2 7C 8E 49 21 01
[24]0A 10 C2 52 6A 86 10

#### MMI_CmdCnf

LLA RRC @ 00:00:15.790

Message Details:

MMI_CmdCnf:

result:true
resultString (IA5String): Omit

#### PHY_DATA_IND

PHY MAC @ 00:00:34.280

BTS unit: 1:1
Channel No: 0 Name: U_RACH
CFN: 89

Message Details:

TFI:0
TB set size:168
TB size:168
TB set (raw):

[0]08 44 48 8C D1 00 04 02
[8]00 02 C0 00 00 00 00 00
[16]00 00 00 00 00 00

TB set (decoded):

TB 0:

TCTF:0
MAC SDU (166 bits):

[0]21 11 22 33 44 00 10 08
[8]00 0B 00 00 00 00 00 00
[16]00 00 00 00 00

#### MAC_DATA_IND

MAC RLC @ 00:00:34.280

Category: Configuration
BTS unit: 1:1
Channel No: 0 Name: CCCH
CFN: 89

Message Details:

RLC PDU size (bits):166
RLC PDU (raw):

[0]21 11 22 33 44 00 10 08
[8]00 0B 00 00 00 00 00 00
[16]00 00 00 00 00

#### RLC_TR_DATA_IND: rrcConnectionRequest

RLC LLA @ 00:00:34.300

Channel No: 0 Name: CCCH

Message Details:

UL_CCCH_Message:

integrityCheckInfo: Omitted

message:

rrcConnectionRequest:

initialUE_Identity:

tmsi_and_LAI:

tmsi: 00010001001000100011001101000100

lai:

plmn_Identity:

mcc:

MCC.element: 0

MCC.element: 0

MCC.element: 1

mnc:

MNC.element: 0

MNC.element: 1

lac: 0000000000000001

establishmentCause: registration_EstablishmentCause [enum=12]

protocolErrorIndicator: noError_ProtocolErrorIndicator [enum=0]

measuredResultsOnRACH: Omitted

v3d0NonCriticalExtensions: Omitted

Layer 3 SDU:

[0]21 11 22 33 44 00 10 08
[8]00 0B 00 00 00 00 00 00
[16]00 00 00 00 00

#### RLC_TR_DATA_IND

LLA RRC @ 00:00:34.300

Channel ID: Rb0
Cell ID: 0

Message Details:

RLC_TR_DATA_IND:

cellId:0

routingInfo:

rB_Identity:0

tM_message:

uL_CCCH_Message:

integrityCheckInfo: Omit

message: (UL_CCCH_MessageType)

rrcConnectionRequest:

initialUE_Identity:

tmsi_and_LAI: (TMSI_and_LAI_GSM_MAP)

tmsi (TMSI_GSM_MAP):00010001001000100011001101000100

lai:

plmn_Identity:

mcc:

Digit:0
Digit:0
Digit:1

mnc:

Digit:0
Digit:1

lac:0000000000000001

establishmentCause:registration
protocolErrorIndicator:noError

measuredResultsOnRACH: Omit

v3d0NonCriticalExtensions: Omit

#### RLC_UM_DATA_REQ

RRC LLA @ 00:00:34.300

Channel ID: Rb0
Cell ID: 0

Message Details:

RLC_UM_DATA_REQ:

cellId:0

routingInfo:

rB_Identity:0

uM_message:

dL_CCCH_Message:

integrityCheckInfo: Omit

message: (DL_CCCH_MessageType)

rrcConnectionSetup:

r3:

rrcConnectionSetup_r3: (RRCConnectionSetup_r3_IEs)

initialUE_Identity:

tmsi_and_LAI: (TMSI_and_LAI_GSM_MAP)

tmsi (TMSI_GSM_MAP):00010001001000100011001101000100

lai:

plmn_Identity:

mcc:

Digit:0
Digit:0
Digit:1

mnc:

Digit:0
Digit:1

lac:0000000000000001

rrc_TransactionIdentifier:0
activationTime: Omit

new_U_RNTI: (U_RNTI)

srnc_Identity:000000000001
s_RNTI:00000000000000000001

new_c_RNTI (C_RNTI): Omit
rrc_StateIndicator:cell_DCH
utran_DRX_CycleLengthCoeff (UTRAN_DRX_CycleLengthCoefficient):9

capabilityUpdateRequirement:

ue_RadioCapabilityFDDUpdateRequirement:true
ue_RadioCapabilityTDDUpdateRequirement:false

systemSpecificCapUpdateReqList:

SystemSpecificCapUpdateReq:gsm

srb_InformationSetupList: (SRB_InformationSetupList2)

SRB_InformationSetup:

rb_Identity: Omit

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_UM_RLC_Mode:

transmissionRLC_Discard: Omit

dl_RLC_Mode:

dl_UM_RLC_Mode:

rb_MappingInfo:

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

dch (TransportChannelIdentity):5

logicalChannelIdentity:1

rlc_SizeList:

configured:

mac_LogicalChannelPriority:1

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

dch (TransportChannelIdentity):10

logicalChannelIdentity:1

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

rach:

logicalChannelIdentity:1

rlc_SizeList:

explicitList: (RLC_SizeExplicitList)

RLC_SizeInfo:

rlc_SizeIndex:1

mac_LogicalChannelPriority:1

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

fach:

logicalChannelIdentity:1

SRB_InformationSetup:

rb_Identity: Omit

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

rb_MappingInfo:

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

dch (TransportChannelIdentity):5

logicalChannelIdentity:2

rlc_SizeList:

configured:

mac_LogicalChannelPriority:2

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

dch (TransportChannelIdentity):10

logicalChannelIdentity:2

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

rach:

logicalChannelIdentity:2

rlc_SizeList:

explicitList: (RLC_SizeExplicitList)

RLC_SizeInfo:

rlc_SizeIndex:1

mac_LogicalChannelPriority:2

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

fach:

logicalChannelIdentity:2

SRB_InformationSetup:

rb_Identity: Omit

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

rb_MappingInfo:

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

dch (TransportChannelIdentity):5

logicalChannelIdentity:3

rlc_SizeList:

configured:

mac_LogicalChannelPriority:3

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

dch (TransportChannelIdentity):10

logicalChannelIdentity:3

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

rach:

logicalChannelIdentity:3

rlc_SizeList:

explicitList: (RLC_SizeExplicitList)

RLC_SizeInfo:

rlc_SizeIndex:1

mac_LogicalChannelPriority:3

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

fach:

logicalChannelIdentity:3

SRB_InformationSetup:

rb_Identity: Omit

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

rb_MappingInfo:

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

dch (TransportChannelIdentity):5

logicalChannelIdentity:4

rlc_SizeList:

configured:

mac_LogicalChannelPriority:4

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

dch (TransportChannelIdentity):10

logicalChannelIdentity:4

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

rach:

logicalChannelIdentity:4

rlc_SizeList:

explicitList: (RLC_SizeExplicitList)

RLC_SizeInfo:

rlc_SizeIndex:1

mac_LogicalChannelPriority:4

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

fach:

logicalChannelIdentity:4

ul_CommonTransChInfo:

tfc_Subset: Omit

prach_TFCS: (TFCS) Omit

modeSpecificInfo:

fdd:

ul_TFCS: (TFCS)

normalTFCI_Signalling: (ExplicitTFCS_Configuration)

complete: (TFCS_ReconfAdd)

ctfcSize:

ctfc2Bit:

:

ctfc2:0

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc2:1

powerOffsetInformation:

gainFactorInformation:

signalledGainFactors:

modeSpecificInfo:

fdd:

gainFactorBetaC (GainFactor):11

gainFactorBetaD (GainFactor):15
referenceTFC_ID:0

powerOffsetPp_m: Omit

ul_AddReconfTransChInfoList:

UL_AddReconfTransChInformation:

ul_TransportChannelType (UL_TrCH_Type):dch
transportChannelIdentity:5

transportFormatSet:

dedicatedTransChTFS:

tti:

tti10: (DedicatedDynamicTF_InfoList)

DedicatedDynamicTF_Info:

rlc_Size:

bitMode: (BitModeRLC_SizeInfo)

sizeType2:

part1:2
part2: Omit

numberOfTbSizeList:

NumberOfTransportBlocks:

zero:

NumberOfTransportBlocks:

one:

logicalChannelList:

allSizes:

semistaticTF_Information:

channelCodingType:

convolutional (CodingRate):third

rateMatchingAttribute:192
crc_Size:crc16

dl_CommonTransChInfo:

sccpch_TFCS: (TFCS) Omit

modeSpecificInfo:

fdd:

dl_Parameters:

sameAsUL:

dl_AddReconfTransChInfoList:

DL_AddReconfTransChInformation:

dl_TransportChannelType (DL_TrCH_Type):dch
dl_transportChannelIdentity (TransportChannelIdentity):10

tfs_SignallingMode:

sameAsULTrCH: (UL_TransportChannelIdentity)

ul_TransportChannelType (UL_TrCH_Type):dch
ul_TransportChannelIdentity (TransportChannelIdentity):5

dch_QualityTarget: (QualityTarget)

bler_QualityValue:-20

dummy: (TM_SignallingInfo) Omit

frequencyInfo: Omit

maxAllowedUL_TX_Power: Omit

ul_ChannelRequirement:

ul_DPCH_Info:

ul_DPCH_PowerControlInfo:

fdd:

dpcch_PowerOffset:-40
pc_Preamble:1
sRB_delay:7

powerControlAlgorithm:

algorithm1 (TPC_StepSizeFDD):1

modeSpecificInfo:

fdd:

scramblingCodeType:longSC
scramblingCode (UL_ScramblingCode):0
numberOfDPDCH: Omit
spreadingFactor:sf64
tfci_Existence:true
numberOfFBI_Bits: Omit
puncturingLimit:pl1

dl_CommonInformation:

dl_DPCH_InfoCommon:

cfnHandling:

initialise:

cfntargetsfnframeoffset: Omit

modeSpecificInfo:

fdd:

dl_DPCH_PowerControlInfo:

modeSpecificInfo:

fdd:

dpc_Mode:singleTPC

powerOffsetPilot_pdpdch:0

dl_rate_matching_restriction: Omit

spreadingFactorAndPilot: (SF512_AndPilot)

sfd128 (PilotBits128):pb4

positionFixedOrFlexible:fixed
tfci_Existence:false

modeSpecificInfo:

fdd:

defaultDPCH_OffsetValue (DefaultDPCH_OffsetValueFDD):0

dpch_CompressedModeInfo: Omit

tx_DiversityMode:noDiversity

ssdt_Information: Omit

dl_InformationPerRL_List:

DL_InformationPerRL:

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode:100

pdsch_SHO_DCH_Info: Omit

pdsch_CodeMapping: Omit

dl_DPCH_InfoPerRL:

fdd:

pCPICH_UsageForChannelEst:mayBeUsed
dpch_FrameOffset:0

secondaryCPICH_Info: Omit

dl_ChannelisationCodeList:

DL_ChannelisationCode:

secondaryScramblingCode:1

sf_AndCodeNumber: (SF512_AndCodeNumber)

sf128:0

scramblingCodeChange:noCodeChange

tpc_CombinationIndex:0
ssdt_CellIdentity: Omit
closedLoopTimingAdjMode: Omit

sccpch_InfoforFACH: Omit

laterNonCriticalExtensions: Omit

specialLI:true

#### RLC_UM_DATA_REQ: rrcConnectionSetup

LLA RLC @ 00:00:34.320

Channel No: 1 Name: CCCH

Message Details:

DL_CCCH_Message:

integrityCheckInfo: Omitted

message:

rrcConnectionSetup:

r3:

rrcConnectionSetup_r3:

initialUE_Identity:

tmsi_and_LAI:

tmsi: 00010001001000100011001101000100

lai:

plmn_Identity:

mcc:

MCC.element: 0

MCC.element: 0

MCC.element: 1

mnc:

MNC.element: 0

MNC.element: 1

lac: 0000000000000001

rrc_TransactionIdentifier: 0

activationTime: Omitted

new_U_RNTI:

srnc_Identity: 000000000001

s_RNTI: 00000000000000000001

new_c_RNTI: Omitted

rrc_StateIndicator: cell_DCH_RRC_StateIndicator [enum=0]

utran_DRX_CycleLengthCoeff: 9

capabilityUpdateRequirement:

ue_RadioCapabilityFDDUpdateRequirement: 1

ue_RadioCapabilityTDDUpdateRequirement: 0

systemSpecificCapUpdateReqList:

SystemSpecificCapUpdateReqList.element: gsm_SystemSpecificCapUpdateReq [enum=0]

srb_InformationSetupList:

SRB_InformationSetupList2.element:

rb_Identity: Omitted

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_UM_RLC_Mode:

transmissionRLC_Discard: Omitted

dl_RLC_Mode:

dl_UM_RLC_Mode: NULL

rb_MappingInfo:

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

dch: 5

logicalChannelIdentity: 1

rlc_SizeList:

configured: NULL

mac_LogicalChannelPriority: 1

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

dch: 10

logicalChannelIdentity: 1

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

rach: NULL

logicalChannelIdentity: 1

rlc_SizeList:

explicitList:

RLC_SizeExplicitList.element:

rlc_SizeIndex: 1

mac_LogicalChannelPriority: 1

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

fach: NULL

logicalChannelIdentity: 1

SRB_InformationSetupList2.element:

rb_Identity: Omitted

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard: dat15_MaxDAT [enum=10]

transmissionWindowSize: tw32_TransmissionWindowSize [enum=3]

timerRST: tr500_TimerRST [enum=9]

max_RST: rst1_MaxRST [enum=0]

pollingInfo:

timerPollProhibit: tpp200_TimerPollProhibit [enum=19]

timerPoll: tp200_TimerPoll [enum=19]

poll_PDU: Omitted

poll_SDU: sdu1_Poll_SDU [enum=0]

lastTransmissionPDU_Poll: 1

lastRetransmissionPDU_Poll: 1

pollWindow: pw99_PollWindow [enum=7]

timerPollPeriodic: Omitted

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery: 1

receivingWindowSize: rw32_ReceivingWindowSize [enum=3]

dl_RLC_StatusInfo:

timerStatusProhibit: tsp200_TimerStatusProhibit [enum=19]

timerEPC: Omitted

missingPDU_Indicator: 1

timerStatusPeriodic: Omitted

rb_MappingInfo:

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

dch: 5

logicalChannelIdentity: 2

rlc_SizeList:

configured: NULL

mac_LogicalChannelPriority: 2

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

dch: 10

logicalChannelIdentity: 2

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

rach: NULL

logicalChannelIdentity: 2

rlc_SizeList:

explicitList:

RLC_SizeExplicitList.element:

rlc_SizeIndex: 1

mac_LogicalChannelPriority: 2

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

fach: NULL

logicalChannelIdentity: 2

SRB_InformationSetupList2.element:

rb_Identity: Omitted

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard: dat15_MaxDAT [enum=10]

transmissionWindowSize: tw32_TransmissionWindowSize [enum=3]

timerRST: tr500_TimerRST [enum=9]

max_RST: rst1_MaxRST [enum=0]

pollingInfo:

timerPollProhibit: tpp200_TimerPollProhibit [enum=19]

timerPoll: tp200_TimerPoll [enum=19]

poll_PDU: Omitted

poll_SDU: sdu1_Poll_SDU [enum=0]

lastTransmissionPDU_Poll: 1

lastRetransmissionPDU_Poll: 1

pollWindow: pw99_PollWindow [enum=7]

timerPollPeriodic: Omitted

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery: 1

receivingWindowSize: rw32_ReceivingWindowSize [enum=3]

dl_RLC_StatusInfo:

timerStatusProhibit: tsp200_TimerStatusProhibit [enum=19]

timerEPC: Omitted

missingPDU_Indicator: 1

timerStatusPeriodic: Omitted

rb_MappingInfo:

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

dch: 5

logicalChannelIdentity: 3

rlc_SizeList:

configured: NULL

mac_LogicalChannelPriority: 3

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

dch: 10

logicalChannelIdentity: 3

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

rach: NULL

logicalChannelIdentity: 3

rlc_SizeList:

explicitList:

RLC_SizeExplicitList.element:

rlc_SizeIndex: 1

mac_LogicalChannelPriority: 3

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

fach: NULL

logicalChannelIdentity: 3

SRB_InformationSetupList2.element:

rb_Identity: Omitted

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard: dat15_MaxDAT [enum=10]

transmissionWindowSize: tw32_TransmissionWindowSize [enum=3]

timerRST: tr500_TimerRST [enum=9]

max_RST: rst1_MaxRST [enum=0]

pollingInfo:

timerPollProhibit: tpp200_TimerPollProhibit [enum=19]

timerPoll: tp200_TimerPoll [enum=19]

poll_PDU: Omitted

poll_SDU: sdu1_Poll_SDU [enum=0]

lastTransmissionPDU_Poll: 1

lastRetransmissionPDU_Poll: 1

pollWindow: pw99_PollWindow [enum=7]

timerPollPeriodic: Omitted

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery: 1

receivingWindowSize: rw32_ReceivingWindowSize [enum=3]

dl_RLC_StatusInfo:

timerStatusProhibit: tsp200_TimerStatusProhibit [enum=19]

timerEPC: Omitted

missingPDU_Indicator: 1

timerStatusPeriodic: Omitted

rb_MappingInfo:

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

dch: 5

logicalChannelIdentity: 4

rlc_SizeList:

configured: NULL

mac_LogicalChannelPriority: 4

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

dch: 10

logicalChannelIdentity: 4

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

rach: NULL

logicalChannelIdentity: 4

rlc_SizeList:

explicitList:

RLC_SizeExplicitList.element:

rlc_SizeIndex: 1

mac_LogicalChannelPriority: 4

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

fach: NULL

logicalChannelIdentity: 4

ul_CommonTransChInfo:

tfc_Subset: Omitted

prach_TFCS: Omitted

modeSpecificInfo:

fdd:

ul_TFCS:

normalTFCI_Signalling:

complete:

ctfcSize:

ctfc2Bit:

ctfc2Bit.noName:

ctfc2: 0

powerOffsetInformation:

gainFactorInformation:

computedGainFactors: 0

powerOffsetPp_m: Omitted

ctfc2Bit.noName:

ctfc2: 1

powerOffsetInformation:

gainFactorInformation:

signalledGainFactors:

modeSpecificInfo:

fdd:

gainFactorBetaC: 11

gainFactorBetaD: 15

referenceTFC_ID: 0

powerOffsetPp_m: Omitted

ul_AddReconfTransChInfoList:

UL_AddReconfTransChInfoList.element:

ul_TransportChannelType: dch_UL_TrCH_Type [enum=0]

transportChannelIdentity: 5

transportFormatSet:

dedicatedTransChTFS:

tti:

tti10:

DedicatedDynamicTF_InfoList.element:

rlc_Size:

bitMode:

sizeType2:

part1: 2

part2: Omitted

numberOfTbSizeList:

numberOfTbSizeList.element:

zero: NULL

numberOfTbSizeList.element:

one: NULL

logicalChannelList:

allSizes: NULL

semistaticTF_Information:

channelCodingType:

convolutional: third_CodingRate [enum=1]

rateMatchingAttribute: 192

crc_Size: crc16_CRC_Size [enum=3]

dl_CommonTransChInfo:

sccpch_TFCS: Omitted

modeSpecificInfo:

fdd:

dl_Parameters:

sameAsUL: NULL

dl_AddReconfTransChInfoList:

DL_AddReconfTransChInfoList.element:

dl_TransportChannelType: dch_DL_TrCH_Type [enum=0]

dl_transportChannelIdentity: 10

tfs_SignallingMode:

sameAsULTrCH:

ul_TransportChannelType: dch_UL_TrCH_Type [enum=0]

ul_TransportChannelIdentity: 5

dch_QualityTarget:

bler_QualityValue: -20

dummy: Omitted

frequencyInfo: Omitted

maxAllowedUL_TX_Power: Omitted

ul_ChannelRequirement:

ul_DPCH_Info:

ul_DPCH_PowerControlInfo:

fdd:

dpcch_PowerOffset: -40

pc_Preamble: 1

sRB_delay: 7

powerControlAlgorithm:

algorithm1: 1

modeSpecificInfo:

fdd:

scramblingCodeType: longSC_ScramblingCodeType [enum=1]

scramblingCode: 0

numberOfDPDCH: Default

spreadingFactor: sf64_SpreadingFactor [enum=4]

tfci_Existence: 1

numberOfFBI_Bits: Omitted

puncturingLimit: pl1_PuncturingLimit [enum=15]

dl_CommonInformation:

dl_DPCH_InfoCommon:

cfnHandling:

initialise:

cfntargetsfnframeoffset: Omitted

modeSpecificInfo:

fdd:

dl_DPCH_PowerControlInfo:

modeSpecificInfo:

fdd:

dpc_Mode: singleTPC_DPC_Mode [enum=0]

powerOffsetPilot_pdpdch: 0

dl_rate_matching_restriction: Omitted

spreadingFactorAndPilot:

sfd128: pb4_PilotBits128 [enum=0]

positionFixedOrFlexible: fixed_PositionFixedOrFlexible [enum=0]

tfci_Existence: 0

modeSpecificInfo:

fdd:

defaultDPCH_OffsetValue: 0

dpch_CompressedModeInfo: Omitted

tx_DiversityMode: noDiversity_TX_DiversityMode [enum=0]

ssdt_Information: Omitted

dl_InformationPerRL_List:

DL_InformationPerRL_List.element:

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode: 100

pdsch_SHO_DCH_Info: Omitted

pdsch_CodeMapping: Omitted

dl_DPCH_InfoPerRL:

fdd:

pCPICH_UsageForChannelEst: mayBeUsed_PCPICH_UsageForChannelEst [enum=0]

dpch_FrameOffset: 0

secondaryCPICH_Info: Omitted

dl_ChannelisationCodeList:

DL_ChannelisationCodeList.element:

secondaryScramblingCode: 1

sf_AndCodeNumber:

sf128: 0

scramblingCodeChange: noCodeChange_ScramblingCodeChange [enum=1]

tpc_CombinationIndex: 0

ssdt_CellIdentity: Omitted

closedLoopTimingAdjMode: Omitted

sccpch_InfoforFACH: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]30 E7 22 24 46 68 80 02
[8]01 00 01 00 04 00 00 4D
[16]82 69 3A 10 10 89 0D 42
[24]00 02 81 9E 8E 46 C9 A6
[32]7C 9C 4E 74 20 A5 12 3A
[40]8C 00 15 13 3D 1C 8D 93
[48]4C F9 38 9C E8 42 52 24
[56]B5 28 00 4A 46 7A 39 1B
[64]26 99 F2 71 39 D0 86 B4
[72]49 EA 70 00 D4 C8 00 06
[80]25 2B F0 02 00 08 82 23
[88]BF 66 08 98 95 A5 47 A2
[96]00 00 01 3F 90 0A 14 00
[104]02 06 40 00 0C 28 08

#### CMAC Configuration REQ

LLA MAC @ 00:00:34.340

BTS unit: 1:1
Channel No: 0 Name: S_CCPCH
CFN: 115

Message Details:

Configuration Parameters:

Number Of Transport Channels:3

Transport Channels:

Item Number 0:

Transport Channel Parameters:

Transport Channel:

Name:PCH
Identity:0

TTI (ms):10
EP Type:1/2 Rate Convolutional Coding
CRC Size:16
RM Attribute:230
First Interleave:On
Number Of Transport Formats:2

Transport Format Set:

Transport Format 0:

Number Of Transport Blocks:0
Transport Block Size In Bits:240

Transport Format 1:

Number Of Transport Blocks:1
Transport Block Size In Bits:240

Number Of Logical Channels:1

Logical Channels:

Item Number 0:

Logical Channel:

Name:PCCH
Identity:0

Priority:1
CT Length:0
CT Value:0
TCTF Length:0
TCTF Value:0
UE ID Type:Not used
UE ID:0

Item Number 1:

Transport Channel Parameters:

Transport Channel:

Name:FACH
Identity:0

TTI (ms):10
EP Type:1/2 Rate Convolutional Coding
CRC Size:16
RM Attribute:220
First Interleave:On
Number Of Transport Formats:3

Transport Format Set:

Transport Format 0:

Number Of Transport Blocks:0
Transport Block Size In Bits:168

Transport Format 1:

Number Of Transport Blocks:1
Transport Block Size In Bits:168

Transport Format 2:

Number Of Transport Blocks:2
Transport Block Size In Bits:168

Number Of Logical Channels:1

Logical Channels:

Item Number 0:

Logical Channel:

Name:CCCH
Identity:1

Priority:1
CT Length:0
CT Value:0
TCTF Length:8
TCTF Value:64
UE ID Type:Not used
UE ID:0

Item Number 2:

Transport Channel Parameters:

Transport Channel:

Name:FACH
Identity:1

TTI (ms):10
EP Type:Turbo Coding
CRC Size:16
RM Attribute:130
First Interleave:On
Number Of Transport Formats:2

Transport Format Set:

Transport Format 0:

Number Of Transport Blocks:0
Transport Block Size In Bits:360

Transport Format 1:

Number Of Transport Blocks:1
Transport Block Size In Bits:360

Number Of Logical Channels:0

Active Flag:1

Transport Format Combination Set:

Number Of Transport Format Combinations:8

Transport Format Combinations 0:

Transport Format:0
Transport Format:0
Transport Format:0

Transport Format Combinations 1:

Transport Format:1
Transport Format:0
Transport Format:0

Transport Format Combinations 2:

Transport Format:0
Transport Format:1
Transport Format:0

Transport Format Combinations 3:

Transport Format:1
Transport Format:1
Transport Format:0

Transport Format Combinations 4:

Transport Format:0
Transport Format:2
Transport Format:0

Transport Format Combinations 5:

Transport Format:1
Transport Format:2
Transport Format:0

Transport Format Combinations 6:

Transport Format:0
Transport Format:0
Transport Format:1

Transport Format Combinations 7:

Transport Format:0
Transport Format:1
Transport Format:1

#### CMAC Configuration CNF

MAC LLA @ 00:00:34.340

BTS unit: 1:1
Channel No: 0 Name: S_CCPCH
CFN: 115

Message Details:

#### MAC_DATA_REQ

RLC MAC @ 00:00:34.350

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: CCCH
CFN: 116

Message Details:

RLC PDU size (bits):160
RLC PDU (raw):

[0]01 F8 30 E7 22 24 46 68
[8]80 02 01 00 01 00 04 00
[16]00 4D 82 69

RLC PDU (decoded):

Sequence number:0
Length indicator 0 (octets):124 (the first data octet in this RLC PDU is the first octet of a RLC SDU)
Segment associated with length indicator 0 (0 octets):

Last segment, not associated with any length indicators (18 octets):

[0]30 E7 22 24 46 68 80 02
[8]01 00 01 00 04 00 00 4D
[16]82 69

#### MAC_DATA_REQ

RLC MAC @ 00:00:34.350

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: CCCH
CFN: 116

Message Details:

RLC PDU size (bits):160
RLC PDU (raw):

[0]02 3A 10 10 89 0D 42 00
[8]02 81 9E 8E 46 C9 A6 7C
[16]9C 4E 74 20

RLC PDU (decoded):

Sequence number:1
Last segment, not associated with any length indicators (19 octets):

[0]3A 10 10 89 0D 42 00 02
[8]81 9E 8E 46 C9 A6 7C 9C
[16]4E 74 20

#### MAC_DATA_REQ

RLC MAC @ 00:00:34.350

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: CCCH
CFN: 116

Message Details:

RLC PDU size (bits):160
RLC PDU (raw):

[0]04 A5 12 3A 8C 00 15 13
[8]3D 1C 8D 93 4C F9 38 9C
[16]E8 42 52 24

RLC PDU (decoded):

Sequence number:2
Last segment, not associated with any length indicators (19 octets):

[0]A5 12 3A 8C 00 15 13 3D
[8]1C 8D 93 4C F9 38 9C E8
[16]42 52 24

#### MAC_DATA_REQ

RLC MAC @ 00:00:34.350

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: CCCH
CFN: 116

Message Details:

RLC PDU size (bits):160
RLC PDU (raw):

[0]06 B5 28 00 4A 46 7A 39
[8]1B 26 99 F2 71 39 D0 86
[16]B4 49 EA 70

RLC PDU (decoded):

Sequence number:3
Last segment, not associated with any length indicators (19 octets):

[0]B5 28 00 4A 46 7A 39 1B
[8]26 99 F2 71 39 D0 86 B4
[16]49 EA 70

#### MAC_DATA_REQ

RLC MAC @ 00:00:34.350

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: CCCH
CFN: 116

Message Details:

RLC PDU size (bits):160
RLC PDU (raw):

[0]08 00 D4 C8 00 06 25 2B
[8]F0 02 00 08 82 23 BF 66
[16]08 98 95 A5

RLC PDU (decoded):

Sequence number:4
Last segment, not associated with any length indicators (19 octets):

[0]00 D4 C8 00 06 25 2B F0
[8]02 00 08 82 23 BF 66 08
[16]98 95 A5

#### MAC_DATA_REQ

RLC MAC @ 00:00:34.350

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: CCCH
CFN: 116

Message Details:

RLC PDU size (bits):160
RLC PDU (raw):

[0]0B 23 FE 47 A2 00 00 01
[8]3F 90 0A 14 00 02 06 40
[16]00 0C 28 08

RLC PDU (decoded):

Sequence number:5
Length indicator 0 (octets):17
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (17 octets):

[0]47 A2 00 00 01 3F 90 0A
[8]14 00 02 06 40 00 0C 28
[16]08
Padding associated with length indicator 1 (0 octets):

#### PHY_DATA_REQ

MAC PHY @ 00:00:34.350

BTS unit: 1:1
Channel No: 0 Name: FACH
CFN: 116

Message Details:

TFI:2
TB set size:336
TB size:168
TB set (raw, each TB word aligned):

[0]40 01 F8 30 E7 22 24 46
[8]68 80 02 01 00 01 00 04
[16]00 00 4D 82 69 00 40 02
[24]3A 10 10 89 0D 42 00 02
[32]81 9E 8E 46 C9 A6 7C 9C
[40]4E 74 20 00

TB set (decoded):

TB 0:

TCTF:64
MAC SDU (160 bits):

[0]01 F8 30 E7 22 24 46 68
[8]80 02 01 00 01 00 04 00
[16]00 4D 82 69

TB 1:

TCTF:64
MAC SDU (160 bits):

[0]02 3A 10 10 89 0D 42 00
[8]02 81 9E 8E 46 C9 A6 7C
[16]9C 4E 74 20

#### PHY_DATA_REQ

MAC PHY @ 00:00:34.360

BTS unit: 1:1
Channel No: 0 Name: FACH
CFN: 117

Message Details:

TFI:2
TB set size:336
TB size:168
TB set (raw, each TB word aligned):

[0]40 04 A5 12 3A 8C 00 15
[8]13 3D 1C 8D 93 4C F9 38
[16]9C E8 42 52 24 00 40 06
[24]B5 28 00 4A 46 7A 39 1B
[32]26 99 F2 71 39 D0 86 B4
[40]49 EA 70 00

TB set (decoded):

TB 0:

TCTF:64
MAC SDU (160 bits):

[0]04 A5 12 3A 8C 00 15 13
[8]3D 1C 8D 93 4C F9 38 9C
[16]E8 42 52 24

TB 1:

TCTF:64
MAC SDU (160 bits):

[0]06 B5 28 00 4A 46 7A 39
[8]1B 26 99 F2 71 39 D0 86
[16]B4 49 EA 70

#### PHY_DATA_REQ

MAC PHY @ 00:00:34.370

BTS unit: 1:1
Channel No: 0 Name: FACH
CFN: 118

Message Details:

TFI:2
TB set size:336
TB size:168
TB set (raw, each TB word aligned):

[0]40 08 00 D4 C8 00 06 25
[8]2B F0 02 00 08 82 23 BF
[16]66 08 98 95 A5 00 40 0B
[24]23 FE 47 A2 00 00 01 3F
[32]90 0A 14 00 02 06 40 00
[40]0C 28 08 00

TB set (decoded):

TB 0:

TCTF:64
MAC SDU (160 bits):

[0]08 00 D4 C8 00 06 25 2B
[8]F0 02 00 08 82 23 BF 66
[16]08 98 95 A5

TB 1:

TCTF:64
MAC SDU (160 bits):

[0]0B 23 FE 47 A2 00 00 01
[8]3F 90 0A 14 00 02 06 40
[16]00 0C 28 08

#### CPHY_SYNC_IND

PHY RRC @ 00:00:34.650

BTS unit: 1:1
Channel No: 0 Name: U_DPCH
CFN: 146

Message Details:

#### PHY_DATA_IND

PHY MAC @ 00:00:34.810

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 142

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 00 04 A0 C0 00 08 00
[8]00 5E 23 41 A2 09 09 8C
[16]D0 8C 50 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 00 4A 0C 00 00 80 00
[8]05 E2 34 1A 20 90 98 CD
[16]08 C5

#### MAC_DATA_IND

MAC RLC @ 00:00:34.810

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 142

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 00 4A 0C 00 00 80 00
[8]05 E2 34 1A 20 90 98 CD
[16]08 C5

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:0
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]4A 0C 00 00 80 00 05 E2
[8]34 1A 20 90 98 CD 08 C5

#### PHY_DATA_IND

PHY MAC @ 00:00:34.820

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 143

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 00 D1 5F E9 26 04 10
[8]00 10 00 23 1F 1F 05 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 0D 15 FE 92 60 41 00
[8]01 00 02 31 F1 F0 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:00:34.820

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 143

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 0D 15 FE 92 60 41 00
[8]01 00 02 31 F1 F0 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:1
Polling bit:1 (request a status report)
Length indicator 0 (octets):10
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (10 octets):

[0]92 60 41 00 01 00 02 31
[8]F1 F0
Padding associated with length indicator 1 (4 octets):

[0]55 55 55 55

#### MAC_DATA_REQ

RLC MAC @ 00:00:34.830

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 164

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 20 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:2

#### PHY_DATA_REQ

MAC PHY @ 00:00:34.830

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 164

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]10 20 02 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]02 00 20 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:00:34.830

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 144

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 00 01 50 08 80 09 82
[8]84 01 00 78 88 00 00 A7
[16]82 FA 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 00 15 00 88 00 98 28
[8]40 10 07 88 80 00 0A 78
[16]2F A0

#### MAC_DATA_IND

MAC RLC @ 00:00:34.830

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 144

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 00 15 00 88 00 98 28
[8]40 10 07 88 80 00 0A 78
[16]2F A0

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:0
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]15 00 88 00 98 28 40 10
[8]07 88 80 00 0A 78 2F A0

#### PHY_DATA_IND

PHY MAC @ 00:00:34.840

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 145

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 00 D1 9F E8 91 19 A2
[8]19 81 A7 8C 40 20 00 04
[16]05 55 50 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 0D 19 FE 89 11 9A 21
[8]98 1A 78 C4 02 00 00 40
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:00:34.840

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 145

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 0D 19 FE 89 11 9A 21
[8]98 1A 78 C4 02 00 00 40
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:1
Polling bit:1 (request a status report)
Length indicator 0 (octets):12
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (12 octets):

[0]89 11 9A 21 98 1A 78 C4
[8]02 00 00 40
Padding associated with length indicator 1 (2 octets):

[0]55 55

#### RLC_AM_DATA_IND: rrcConnectionSetupComplete

RLC LLA @ 00:00:34.850

Channel No: 2 Name: DCCH

Message Details:

UL_DCCH_Message:

integrityCheckInfo: Omitted

message:

rrcConnectionSetupComplete:

rrc_TransactionIdentifier: 0

startList:

STARTList.element:

cn_DomainIdentity: ps_domain_CN_DomainIdentity [enum=1]

start_Value: 00000000000000000010

STARTList.element:

cn_DomainIdentity: cs_domain_CN_DomainIdentity [enum=0]

start_Value: 00000000000000000010

ue_RadioAccessCapability:

accessStratumReleaseIndicator: r99_AccessStratumReleaseIndicator [enum=0]

pdcp_Capability:

losslessSRNS_RelocationSupport: 1

supportForRfc2507:

supported: by8192_MaxHcContextSpace [enum=4]

rlc_Capability:

totalRLC_AM_BufferSize: kb50_TotalRLC_AM_BufferSize [enum=2]

maximumRLC_WindowSize: mws2047_MaximumRLC_WindowSize [enum=0]

maximumAM_EntityNumber: am6_MaximumAM_EntityNumberRLC_Cap [enum=3]

transportChannelCapability:

dl_TransChCapability:

maxNoBitsReceived: b5120_MaxNoBits [enum=4]

maxConvCodeBitsReceived: b1280_MaxNoBits [enum=1]

turboDecodingSupport:

supported: b5120_MaxNoBits [enum=4]

maxSimultaneousTransChs: e8_MaxSimultaneousTransChsDL [enum=1]

maxSimultaneousCCTrCH_Count: 1

maxReceivedTransportBlocks: tb16_MaxTransportBlocksDL [enum=2]

maxNumberOfTFC: tfc96_MaxNumberOfTFC_DL [enum=4]

maxNumberOfTF: tf64_MaxNumberOfTF [enum=1]

ul_TransChCapability:

maxNoBitsTransmitted: b3840_MaxNoBits [enum=3]

maxConvCodeBitsTransmitted: b1280_MaxNoBits [enum=1]

turboEncodingSupport:

supported: b3840_MaxNoBits [enum=3]

maxSimultaneousTransChs: e8_MaxSimultaneousTransChsUL [enum=2]

modeSpecificInfo:

fdd: NULL

maxTransmittedBlocks: tb8_MaxTransportBlocksUL [enum=2]

maxNumberOfTFC: tfc32_MaxNumberOfTFC_UL [enum=3]

maxNumberOfTF: tf32_MaxNumberOfTF [enum=0]

rf_Capability:

fddRF_Capability:

ue_PowerClass: 4

txRxFrequencySeparation: mhz190_TxRxFrequencySeparation [enum=0]

tddRF_Capability: Omitted

physicalChannelCapability:

fddPhysChCapability:

downlinkPhysChCapability:

maxNoDPCH_PDSCH_Codes: 3

maxNoPhysChBitsReceived: b9600_MaxNoPhysChBitsReceived [enum=6]

supportForSF_512: 0

supportOfPDSCH: 0

simultaneousSCCPCH_DPCH_Reception:

notSupported: NULL

uplinkPhysChCapability:

maxNoDPDCH_BitsTransmitted: b2400_MaxNoDPDCH_BitsTransmitted [enum=2]

supportOfPCPCH: 0

tddPhysChCapability: Omitted

ue_MultiModeRAT_Capability:

multiRAT_CapabilityList:

supportOfGSM: 0

supportOfMulticarrier: 0

multiModeCapability: fdd_MultiModeCapability [enum=1]

securityCapability:

cipheringAlgorithmCap: 0000000000000001

integrityProtectionAlgorithmCap: 0000000000000010

ue_positioning_Capability:

standaloneLocMethodsSupported: 0

ue_BasedOTDOA_Supported: 0

networkAssistedGPS_Supported: noNetworkAssistedGPS_NetworkAssistedGPS_Supported [enum=3]

supportForUE_GPS_TimingOfCellFrames: 0

supportForIPDL: 0

measurementCapability:

downlinkCompressedMode:

fdd_Measurements: 1

tdd_Measurements: Omitted

gsm_Measurements:

gsm900: 1

dcs1800: 1

gsm1900: 0

multiCarrierMeasurements: 0

uplinkCompressedMode:

fdd_Measurements: 1

tdd_Measurements: Omitted

gsm_Measurements:

gsm900: 1

dcs1800: 1

gsm1900: 0

multiCarrierMeasurements: 0

ue_RATSpecificCapability: Omitted

v370NonCriticalExtensions: Omitted

Layer 3 SDU:

[0]4A 0C 00 00 80 00 05 E2
[8]34 1A 20 90 98 CD 08 C5
[16]92 60 41 00 01 00 02 31
[24]F1 F0

#### MAC_DATA_REQ

RLC MAC @ 00:00:34.850

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 166

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 20 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:2

#### PHY_DATA_REQ

MAC PHY @ 00:00:34.850

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 166

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 02 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 20 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### RLC_AM_DATA_IND

LLA RRC @ 00:00:34.860

Channel ID: Rb2
Cell ID: -1

Message Details:

RLC_AM_DATA_IND:

cellId:-1

routingInfo:

rB_Identity:2

integrityResult:

integrityUsed (IntegrityStatus):i_pass

aM_message:

uL_DCCH_Message:

integrityCheckInfo: Omit

message: (UL_DCCH_MessageType)

rrcConnectionSetupComplete:

rrc_TransactionIdentifier:0

startList:

STARTSingle:

cn_DomainIdentity:ps_domain
start_Value:00000000000000000010

STARTSingle:

cn_DomainIdentity:cs_domain
start_Value:00000000000000000010

ue_RadioAccessCapability:

accessStratumReleaseIndicator:r99

pdcp_Capability:

losslessSRNS_RelocationSupport:true

supportForRfc2507:

supported (MaxHcContextSpace):by8192

rlc_Capability:

totalRLC_AM_BufferSize:kb50
maximumRLC_WindowSize:mws2047
maximumAM_EntityNumber (MaximumAM_EntityNumberRLC_Cap):am6

transportChannelCapability:

dl_TransChCapability:

maxNoBitsReceived (MaxNoBits):b5120
maxConvCodeBitsReceived (MaxNoBits):b1280

turboDecodingSupport: (TurboSupport)

supported (MaxNoBits):b5120

maxSimultaneousTransChs (MaxSimultaneousTransChsDL):e8
maxSimultaneousCCTrCH_Count:1
maxReceivedTransportBlocks (MaxTransportBlocksDL):tb16
maxNumberOfTFC (MaxNumberOfTFC_DL):tfc96
maxNumberOfTF:tf64

ul_TransChCapability:

maxNoBitsTransmitted (MaxNoBits):b3840
maxConvCodeBitsTransmitted (MaxNoBits):b1280

turboEncodingSupport: (TurboSupport)

supported (MaxNoBits):b3840

maxSimultaneousTransChs (MaxSimultaneousTransChsUL):e8

modeSpecificInfo:

fdd:

maxTransmittedBlocks (MaxTransportBlocksUL):tb8
maxNumberOfTFC (MaxNumberOfTFC_UL):tfc32
maxNumberOfTF:tf32

rf_Capability:

fddRF_Capability:

ue_PowerClass:4
txRxFrequencySeparation:mhz190

tddRF_Capability: Omit

physicalChannelCapability:

fddPhysChCapability:

downlinkPhysChCapability: (DL_PhysChCapabilityFDD)

maxNoDPCH_PDSCH_Codes:3
maxNoPhysChBitsReceived:b9600
supportForSF_512:false
supportOfPDSCH:false

simultaneousSCCPCH_DPCH_Reception:

notSupported:

uplinkPhysChCapability: (UL_PhysChCapabilityFDD)

maxNoDPDCH_BitsTransmitted:b2400
supportOfPCPCH:false

tddPhysChCapability: Omit

ue_MultiModeRAT_Capability:

multiRAT_CapabilityList: (MultiRAT_Capability)

supportOfGSM:false
supportOfMulticarrier:false

multiModeCapability:fdd

securityCapability:

cipheringAlgorithmCap:0000000000000001
integrityProtectionAlgorithmCap:0000000000000010

ue_positioning_Capability:

standaloneLocMethodsSupported:false
ue_BasedOTDOA_Supported:false
networkAssistedGPS_Supported:noNetworkAssistedGPS
supportForUE_GPS_TimingOfCellFrames:false
supportForIPDL:false

measurementCapability:

downlinkCompressedMode: (CompressedModeMeasCapability)

fdd_Measurements:true
tdd_Measurements: Omit

gsm_Measurements:

gsm900:true
dcs1800:true
gsm1900:false

multiCarrierMeasurements:false

uplinkCompressedMode: (CompressedModeMeasCapability)

fdd_Measurements:true
tdd_Measurements: Omit

gsm_Measurements:

gsm900:true
dcs1800:true
gsm1900:false

multiCarrierMeasurements:false

ue_RATSpecificCapability: (InterRAT_UE_RadioAccessCapabilityList) Omit

v370NonCriticalExtensions: Omit

#### RLC_AM_DATA_IND: initialDirectTransfer

RLC RRC @ 00:00:34.850

Channel No: 3 Name: DCCH

Message Details:

UL_DCCH_Message:

integrityCheckInfo: Omitted

message:

initialDirectTransfer:

cn_DomainIdentity: cs_domain_CN_DomainIdentity [enum=0]

intraDomainNasNodeSelector:

version:

release99:

cn_Type:

gsm_Map_IDNNS:

routingbasis:

localPTMSI:

routingparameter: 0010001000

enteredparameter: 0

nas_Message: 05080200F11000014F05F41122334433034F1880

measuredResultsOnRACH: Omitted

v3a0NonCriticalExtensions:

initialDirectTransfer_v3a0ext:

start_Value: 00000000000000000010

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]15 00 88 00 98 28 40 10
[8]07 88 80 00 0A 78 2F A0
[16]89 11 9A 21 98 1A 78 C4
[24]02 00 00 40

#### RRC_DATA_IND: mm:locationUpdatingRequest

RRC NAS @ 00:00:34.850

Cell ID: -1

Message Details:

LOCATIONUPDATINGREQUEST:

skipIndicator: 0000

mMProtocolDiscriminator: 0101

msgType: 00001000

ciphKeySeqNum:

spare1: 0

keySeq: 000

locUpdType:

fOR: 0

spare1: 0

lUT: 10

locAreaId:

plmn: 00F110

lac: 0001

mSClsmk1:

spare1: 0

revLvl: 10

eSIND: 0

a5_1: 1

rFPwrCap: 111

mobileId:

iel: 05

iDigit1: 1111

oddEvenInd: 0

typeOfId: 100

otherDigits: 11223344

mSClsmk2:

iei: 00110011

iel: 03

spare1_1: 0

revLvl: 10

eSIND: 0

a5_1: 1

rFPwrCap: 111

spare1_2: 0

pSCap: 0

sSSI: 01

sMCap: 1

vBS: 0

vGCS: 0

fC: 0

cM3: 1

spare1_3: 0

lCSVA: 0

uCS2: 0

soLSA: 0

cMSP: 0

a5_3: 0

a5_2: 0

#### RRC_DATA_REQ: mm:authenticationRequest

NAS RRC @ 00:00:34.900

Cell ID: -1

Message Details:

AUTHENTICATIONREQUEST:

skipIndicator: 0000

mMProtocolDiscriminator: 0101

msgType: 00010010

spare4: 0000

ciphKeySeqNum:

spare1: 0

keySeq: 000

rAND: 01010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101

aUTN:

iei: 00100000

iel: 10

aUTN: 01100110000100010000000000110011001000101101110100000000000000000101010101000100011101110110011000010001000000000011001100100010

#### RLC_AM_DATA_REQ:downlinkDirectTransfer

RRC RLC @ 00:00:34.900

Channel No: 3 Name: DCCH

Message Details:

Opt1: 0

Opt2: 0

DL_DCCH_Message:

integrityCheckInfo: Omitted

message:

downlinkDirectTransfer:

r3:

downlinkDirectTransfer_r3:

rrc_TransactionIdentifier: 0

cn_DomainIdentity: cs_domain_CN_DomainIdentity [enum=0]

nas_Message: 0512005555555555555555555555555555555520106611003322DD00005544776611003322

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]14 00 48 0A 24 00 AA AA
[8]AA AA AA AA AA AA AA AA
[16]AA AA AA AA AA AA 40 20
[24]CC 22 00 66 45 BA 00 00
[32]AA 88 EE CC 22 00 66 44

#### MAC_DATA_REQ

RLC MAC @ 00:00:34.950

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 176

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 00 14 00 48 0A 24 00
[8]AA AA AA AA AA AA AA AA
[16]AA AA

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:0
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]14 00 48 0A 24 00 AA AA
[8]AA AA AA AA AA AA AA AA

#### MAC_DATA_REQ

RLC MAC @ 00:00:34.950

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 176

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 08 AA AA AA AA AA AA
[8]40 20 CC 22 00 66 45 BA
[16]00 00

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:1
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]AA AA AA AA AA AA 40 20
[8]CC 22 00 66 45 BA 00 00

#### MAC_DATA_REQ

RLC MAC @ 00:00:34.950

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 176

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 15 11 FE AA 88 EE CC
[8]22 00 66 44 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:2
Polling bit:1 (request a status report)
Length indicator 0 (octets):8
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (8 octets):

[0]AA 88 EE CC 22 00 66 44
Padding associated with length indicator 1 (6 octets):

[0]00 00 00 00 00 00

#### PHY_DATA_REQ

MAC PHY @ 00:00:34.950

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 176

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 00 01 40 04 80 A2 40
[8]0A AA AA AA AA AA AA AA
[16]AA AA A0 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 00 14 00 48 0A 24 00
[8]AA AA AA AA AA AA AA AA
[16]AA AA

#### PHY_DATA_REQ

MAC PHY @ 00:00:34.960

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 177

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 00 8A AA AA AA AA AA
[8]A4 02 0C C2 20 06 64 5B
[16]A0 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 08 AA AA AA AA AA AA
[8]40 20 CC 22 00 66 45 BA
[16]00 00

#### PHY_DATA_REQ

MAC PHY @ 00:00:34.970

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 178

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 01 51 1F EA A8 8E EC
[8]C2 20 06 64 40 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 15 11 FE AA 88 EE CC
[8]22 00 66 44 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:00:35.030

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 164

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 00 D1 5F E9 26 04 10
[8]00 10 00 23 1F 1F 05 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 0D 15 FE 92 60 41 00
[8]01 00 02 31 F1 F0 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:00:35.030

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 164

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 0D 15 FE 92 60 41 00
[8]01 00 02 31 F1 F0 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:1
Polling bit:1 (request a status report)
Length indicator 0 (octets):10
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (10 octets):

[0]92 60 41 00 01 00 02 31
[8]F1 F0
Padding associated with length indicator 1 (4 octets):

[0]55 55 55 55

#### MAC_DATA_REQ

RLC MAC @ 00:00:35.040

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 185

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 20 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:2

#### PHY_DATA_REQ

MAC PHY @ 00:00:35.040

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 185

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]10 20 02 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]02 00 20 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:00:35.050

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 166

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 00 D1 9F E8 91 19 A2
[8]19 81 A7 8C 40 20 00 04
[16]05 55 50 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 0D 19 FE 89 11 9A 21
[8]98 1A 78 C4 02 00 00 40
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:00:35.050

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 166

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 0D 19 FE 89 11 9A 21
[8]98 1A 78 C4 02 00 00 40
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:1
Polling bit:1 (request a status report)
Length indicator 0 (octets):12
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (12 octets):

[0]89 11 9A 21 98 1A 78 C4
[8]02 00 00 40
Padding associated with length indicator 1 (2 octets):

[0]55 55

#### MAC_DATA_REQ

RLC MAC @ 00:00:35.060

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 187

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 20 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:2

#### PHY_DATA_REQ

MAC PHY @ 00:00:35.060

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 187

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 02 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 20 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### MAC_DATA_REQ

RLC MAC @ 00:00:35.150

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 196

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 15 11 FE AA 88 EE CC
[8]22 00 66 44 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:2
Polling bit:1 (request a status report)
Length indicator 0 (octets):8
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (8 octets):

[0]AA 88 EE CC 22 00 66 44
Padding associated with length indicator 1 (6 octets):

[0]00 00 00 00 00 00

#### PHY_DATA_REQ

MAC PHY @ 00:00:35.150

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 196

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 01 51 1F EA A8 8E EC
[8]C2 20 06 64 40 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 15 11 FE AA 88 EE CC
[8]22 00 66 44 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:00:35.210

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 182

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 03 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### MAC_DATA_IND

MAC RLC @ 00:00:35.210

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 182

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:3

#### PHY_DATA_IND

PHY MAC @ 00:00:35.300

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 191

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 01 06 C0 09 82 AA 2A
[8]A2 3B B3 10 86 08 80 19
[16]91 6E E0 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 10 6C 00 98 2A A2 AA
[8]23 BB 31 08 60 88 01 99
[16]16 EE

#### MAC_DATA_IND

MAC RLC @ 00:00:35.300

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 191

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 10 6C 00 98 2A A2 AA
[8]23 BB 31 08 60 88 01 99
[16]16 EE

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:2
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]6C 00 98 2A A2 AA 23 BB
[8]31 08 60 88 01 99 16 EE

#### PHY_DATA_IND

PHY MAC @ 00:00:35.310

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 192

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 01 D0 FF E6 7F F7 4C
[8]C4 5D D5 05 55 55 55 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 1D 0F FE 67 FF 74 CC
[8]45 DD 50 55 55 55 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:00:35.310

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 192

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 1D 0F FE 67 FF 74 CC
[8]45 DD 50 55 55 55 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:3
Polling bit:1 (request a status report)
Length indicator 0 (octets):7
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (7 octets):

[0]67 FF 74 CC 45 DD 50
Padding associated with length indicator 1 (7 octets):

[0]55 55 55 55 55 55 55

#### RLC_AM_DATA_IND: uplinkDirectTransfer

RLC RRC @ 00:00:35.320

Channel No: 3 Name: DCCH

Message Details:

UL_DCCH_Message:

integrityCheckInfo: Omitted

message:

uplinkDirectTransfer:

cn_DomainIdentity: cs_domain_CN_DomainIdentity [enum=0]

nas_Message: 055455447766210C11003322DDCCFFEE9988BBAA

measuredResultsOnRACH: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]6C 00 98 2A A2 AA 23 BB
[8]31 08 60 88 01 99 16 EE
[16]67 FF 74 CC 45 DD 50

#### RRC_DATA_IND: mm:authenticationResponse

RRC NAS @ 00:00:35.320

Cell ID: -1

Message Details:

AUTHENTICATIONRESPONSE:

skipIndicator: 0000

mMProtocolDiscriminator: 0101

msgType: 01010100

authRsp: 01010101010001000111011101100110

authRspExt:

iei: 00100001

iel: 0C

rES: 000100010000000000110011001000101101110111001100111111111110111010011001100010001011101110101010

#### MAC_DATA_REQ

RLC MAC @ 00:00:35.320

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 213

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 40 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:4

#### PHY_DATA_REQ

MAC PHY @ 00:00:35.320

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 213

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 04 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 40 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### CRLC_SecurityMode_Config_REQ

RRC LLA @ 00:00:35.350

Cell ID: -1

Message Details:

CRLC_SecurityMode_Config_REQ:

cellId:-1

rlcSecurityInfo: (SecurityInfo)

cn_DomainIdentity:cs_domain
startValue (START_Value):00000000000000000000
cipheringKey: Omit
integrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
gsmCipheringKey: Omit

#### CRLC_SecurityMode_Config_REQ

RRC RLC @ 00:00:35.350

Message Details:

cellIdentity: 1

rlcSecurityInfo:

cn_DomainIdentity: cs_domain_CN_DomainIdentity

startValue: 00000000000000000000

cipheringKey: Omitted

integrityKey: 01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100

#### CRLC_SecurityMode_Config_CNF

LLA RRC @ 00:00:35.360

Cell ID: -1

Message Details:

CRLC_SecurityMode_Config_CNF:

cellId:-1

#### CRLC_SetRRC_MessageSN_REQ

RRC LLA @ 00:00:35.360

Channel ID: Rb0
Cell ID: 0

Message Details:

CRLC_SetRRC_MessageSN_REQ:

cellId:0

routingInfo:

rB_Identity:0

count_I_LSB_UL (RRC_SequenceNumber): Omit
count_I_LSB_DL (RRC_SequenceNumber):0

#### CRLC_SetRRC_MessageSN_CNF

LLA RRC @ 00:00:35.380

Channel ID: Rb0
Cell ID: 0

Message Details:

CRLC_SetRRC_MessageSN_CNF:

cellId:0

routingInfo:

rB_Identity:0

#### CRLC_SetRRC_MessageSN_REQ

RRC LLA @ 00:00:35.380

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_REQ:

cellId:-1

routingInfo:

rB_Identity:1

count_I_LSB_UL (RRC_SequenceNumber): Omit
count_I_LSB_DL (RRC_SequenceNumber):0

#### CRLC_SetRRC_MessageSN_CNF

LLA RRC @ 00:00:35.400

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_CNF:

cellId:-1

routingInfo:

rB_Identity:1

#### CRLC_SetRRC_MessageSN_REQ

RRC LLA @ 00:00:35.400

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_REQ:

cellId:-1

routingInfo:

rB_Identity:2

count_I_LSB_UL (RRC_SequenceNumber): Omit
count_I_LSB_DL (RRC_SequenceNumber):0

#### PHY_DATA_IND

PHY MAC @ 00:00:35.410

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 202

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 03 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### MAC_DATA_IND

MAC RLC @ 00:00:35.410

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 202

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:3

#### CRLC_SetRRC_MessageSN_CNF

LLA RRC @ 00:00:35.410

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_CNF:

cellId:-1

routingInfo:

rB_Identity:2

#### CRLC_SetRRC_MessageSN_REQ

RRC LLA @ 00:00:35.410

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_REQ:

cellId:-1

routingInfo:

rB_Identity:3

count_I_LSB_UL (RRC_SequenceNumber): Omit
count_I_LSB_DL (RRC_SequenceNumber):0

#### CRLC_SetRRC_MessageSN_CNF

LLA RRC @ 00:00:35.430

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_CNF:

cellId:-1

routingInfo:

rB_Identity:3

#### CRLC_SetRRC_MessageSN_REQ

RRC LLA @ 00:00:35.430

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_REQ:

cellId:-1

routingInfo:

rB_Identity:4

count_I_LSB_UL (RRC_SequenceNumber): Omit
count_I_LSB_DL (RRC_SequenceNumber):0

#### CRLC_SetRRC_MessageSN_CNF

LLA RRC @ 00:00:35.440

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_CNF:

cellId:-1

routingInfo:

rB_Identity:4

#### CRLC_Integrity_Activate_REQ

RRC LLA @ 00:00:35.440

Cell ID: -1

Message Details:

CRLC_Integrity_Activate_REQ:

cellId:-1
cn_DomainIdentity:cs_domain

integrityActivationInfo:

integrityProtectionModeInfo:

integrityProtectionModeCommand:

startIntegrityProtection:

integrityProtInitNumber:00001111000011110000111100001111

integrityProtectionAlgorithm:uia1

#### CRLC_Integrity_Activate_REQ

RRC RLC @ 00:00:35.440

Message Details:

cellIdentity: 1

integrityActivationInfo:

integrityProtectionModeInfo:

integrityProtectionModeCommand:

startIntegrityProtection:

integrityProtInitNumber: 00001111000011110000111100001111

#### CRLC_Integrity_Activate_CNF

LLA RRC @ 00:00:35.460

Cell ID: -1

Message Details:

CRLC_Integrity_Activate_CNF:

cellId:-1

#### CRLC_Integrity_Activate_REQ

RRC LLA @ 00:00:35.460

Cell ID: -1

Message Details:

CRLC_Integrity_Activate_REQ:

cellId:-1
cn_DomainIdentity:cs_domain

integrityActivationInfo:

ul_IntegProtActivationInfo: (IntegrityProtActivationInfoList)

SS_IntegrityProtActivationTimeInfo:

rb_Identity:2
rrc_MessageSequenceNumber:0

#### CMAC Integrity Check Request

RRC MAC @ 00:00:35.470

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000001
Data:

[0]00 00 00 01
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:1 (RNC to UE)
Message Length (bits):120
Message:

[0]80 00 00 01 04 04 00 00
[8]80 01 41 E1 E1 E1 E0

#### CMAC Integrity Check Result

MAC RRC @ 00:00:35.470

Message Details:

Integrity Check Result:

MAC-I:10000110000011011010000010001001
Data:

[0]86 0D A0 89

#### CRLC_Integrity_Activate_CNF

LLA RRC @ 00:00:35.470

Cell ID: -1

Message Details:

CRLC_Integrity_Activate_CNF:

cellId:-1

#### RLC_AM_DATA_REQ

RRC LLA @ 00:00:35.470

Channel ID: Rb2
Cell ID: -1

Message Details:

RLC_AM_DATA_REQ:

cellId:-1

routingInfo:

rB_Identity:2

confirmationRequest: (AmConfirmationRequest)

noConfirmationRequest:

aM_message:

dL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode:00000000000000000000000000000000
rrc_MessageSequenceNumber:0

message: (DL_DCCH_MessageType)

securityModeCommand:

r3:

securityModeCommand_r3: (SecurityModeCommand_r3_IEs)

rrc_TransactionIdentifier:0

securityCapability:

cipheringAlgorithmCap:0000000000000001
integrityProtectionAlgorithmCap:0000000000000010

cipheringModeInfo: Omit

integrityProtectionModeInfo:

integrityProtectionModeCommand:

startIntegrityProtection:

integrityProtInitNumber:00001111000011110000111100001111

integrityProtectionAlgorithm:uia1

cn_DomainIdentity:cs_domain

ue_SystemSpecificSecurityCap: (InterRAT_UE_SecurityCapList) Omit

laterNonCriticalExtensions: Omit

#### RLC_AM_DATA_REQ: securityModeCommand

LLA RLC @ 00:00:35.470

Channel No: 2 Name: DCCH

Message Details:

DL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode: 10000110000011011010000010001001

rrc_MessageSequenceNumber: 1

message:

securityModeCommand:

r3:

securityModeCommand_r3:

rrc_TransactionIdentifier: 0

securityCapability:

cipheringAlgorithmCap: 0000000000000001

integrityProtectionAlgorithmCap: 0000000000000010

cipheringModeInfo: Omitted

integrityProtectionModeInfo:

integrityProtectionModeCommand:

startIntegrityProtection:

integrityProtInitNumber: 00001111000011110000111100001111

integrityProtectionAlgorithm: uia1_IntegrityProtectionAlgorithm [enum=0]

cn_DomainIdentity: cs_domain_CN_DomainIdentity [enum=0]

ue_SystemSpecificSecurityCap: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]C3 06 D0 44 8C 04 00 00
[8]80 01 41 E1 E1 E1 E0

#### PHY_DATA_IND

PHY MAC @ 00:00:35.510

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 212

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 01 D0 FF E6 7F F7 4C
[8]C4 5D D5 05 55 55 55 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 1D 0F FE 67 FF 74 CC
[8]45 DD 50 55 55 55 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:00:35.510

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 212

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 1D 0F FE 67 FF 74 CC
[8]45 DD 50 55 55 55 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:3
Polling bit:1 (request a status report)
Length indicator 0 (octets):7
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (7 octets):

[0]67 FF 74 CC 45 DD 50
Padding associated with length indicator 1 (7 octets):

[0]55 55 55 55 55 55 55

#### MAC_DATA_REQ

RLC MAC @ 00:00:35.520

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 233

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 40 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:4

#### PHY_DATA_REQ

MAC PHY @ 00:00:35.520

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 233

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 04 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 40 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### MAC_DATA_REQ

RLC MAC @ 00:00:35.530

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 234

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 05 1E C3 06 D0 44 8C
[8]04 00 00 80 01 41 E1 E1
[16]E1 E0

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:0
Polling bit:1 (request a status report)
Length indicator 0 (octets):15
Segment associated with length indicator 0 (15 octets):

[0]C3 06 D0 44 8C 04 00 00
[8]80 01 41 E1 E1 E1 E0

#### PHY_DATA_REQ

MAC PHY @ 00:00:35.530

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 234

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 00 51 EC 30 6D 04 48
[8]C0 40 00 08 00 14 1E 1E
[16]1E 1E 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 05 1E C3 06 D0 44 8C
[8]04 00 00 80 01 41 E1 E1
[16]E1 E0

#### MAC_DATA_REQ

RLC MAC @ 00:00:35.730

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 254

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 05 1E C3 06 D0 44 8C
[8]04 00 00 80 01 41 E1 E1
[16]E1 E0

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:0
Polling bit:1 (request a status report)
Length indicator 0 (octets):15
Segment associated with length indicator 0 (15 octets):

[0]C3 06 D0 44 8C 04 00 00
[8]80 01 41 E1 E1 E1 E0

#### PHY_DATA_REQ

MAC PHY @ 00:00:35.730

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 254

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 00 51 EC 30 6D 04 48
[8]C0 40 00 08 00 14 1E 1E
[16]1E 1E 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 05 1E C3 06 D0 44 8C
[8]04 00 00 80 01 41 E1 E1
[16]E1 E0

#### PHY_DATA_IND

PHY MAC @ 00:00:35.770

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 238

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]10 20 01 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]02 00 10 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### MAC_DATA_IND

MAC RLC @ 00:00:35.770

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 238

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 10 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:1

#### PHY_DATA_IND

PHY MAC @ 00:00:35.780

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 239

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 01 51 3F EC 59 1B E7
[8]10 D2 10 00 00 05 55 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 15 13 FE C5 91 BE 71
[8]0D 21 00 00 00 55 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:00:35.780

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 239

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 15 13 FE C5 91 BE 71
[8]0D 21 00 00 00 55 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:2
Polling bit:1 (request a status report)
Length indicator 0 (octets):9
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (9 octets):

[0]C5 91 BE 71 0D 21 00 00
[8]00
Padding associated with length indicator 1 (5 octets):

[0]55 55 55 55 55

#### MAC_DATA_REQ

RLC MAC @ 00:00:35.790

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 4

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:3

#### PHY_DATA_REQ

MAC PHY @ 00:00:35.790

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 4

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]10 20 03 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:00:35.970

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 2

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]10 20 01 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]02 00 10 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### MAC_DATA_IND

MAC RLC @ 00:00:35.970

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 2

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 10 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:1

#### PHY_DATA_IND

PHY MAC @ 00:00:35.980

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 3

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 01 51 3F EC 59 1B E7
[8]10 D2 10 00 00 05 55 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 15 13 FE C5 91 BE 71
[8]0D 21 00 00 00 55 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:00:35.980

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 3

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 15 13 FE C5 91 BE 71
[8]0D 21 00 00 00 55 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:2
Polling bit:1 (request a status report)
Length indicator 0 (octets):9
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (9 octets):

[0]C5 91 BE 71 0D 21 00 00
[8]00
Padding associated with length indicator 1 (5 octets):

[0]55 55 55 55 55

#### MAC_DATA_REQ

RLC MAC @ 00:00:35.990

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 24

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:3

#### PHY_DATA_REQ

MAC PHY @ 00:00:35.990

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 24

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]10 20 03 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### CMAC Integrity Check Request

RRC MAC @ 00:00:36.050

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000001
Data:

[0]00 00 00 01
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:0 (UE to RNC)
Message Length (bits):72
Message:

[0]80 00 00 01 05 21 00 00
[8]00

#### RLC_AM_DATA_IND: securityModeComplete

RLC LLA @ 00:00:36.050

Channel No: 2 Name: DCCH

Message Details:

UL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode: 10001011001000110111110011100010

rrc_MessageSequenceNumber: 1

message:

securityModeComplete:

rrc_TransactionIdentifier: 0

ul_IntegProtActivationInfo:

rrc_MessageSequenceNumberList:

RRC_MessageSequenceNumberList.element: 0

RRC_MessageSequenceNumberList.element: 0

RRC_MessageSequenceNumberList.element: 0

RRC_MessageSequenceNumberList.element: 0

RRC_MessageSequenceNumberList.element: 0

rb_UL_CiphActivationTimeInfo: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]C5 91 BE 71 0D 21 00 00
[8]00

#### CMAC Integrity Check Result

MAC RRC @ 00:00:36.050

Message Details:

Integrity Check Result:

MAC-I:10001011001000110111110011100010
Data:

[0]8B 23 7C E2

#### RLC_AM_DATA_IND

LLA RRC @ 00:00:36.050

Channel ID: Rb2
Cell ID: -1

Message Details:

RLC_AM_DATA_IND:

cellId:-1

routingInfo:

rB_Identity:2

integrityResult:

integrityUsed (IntegrityStatus):i_pass

aM_message:

uL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode:10001011001000110111110011100010
rrc_MessageSequenceNumber:1

message: (UL_DCCH_MessageType)

securityModeComplete:

rrc_TransactionIdentifier:0

ul_IntegProtActivationInfo: (IntegrityProtActivationInfo)

rrc_MessageSequenceNumberList:

RRC_MessageSequenceNumber:0
RRC_MessageSequenceNumber:0
RRC_MessageSequenceNumber:0
RRC_MessageSequenceNumber:0
RRC_MessageSequenceNumber:0

rb_UL_CiphActivationTimeInfo: (RB_ActivationTimeInfoList) Omit

laterNonCriticalExtensions: Omit

#### CRLC_Integrity_Activate_REQ

RRC LLA @ 00:00:36.050

Cell ID: -1

Message Details:

CRLC_Integrity_Activate_REQ:

cellId:-1
cn_DomainIdentity:cs_domain

integrityActivationInfo:

ul_IntegProtActivationInfo: (IntegrityProtActivationInfoList)

SS_IntegrityProtActivationTimeInfo:

rb_Identity:0
rrc_MessageSequenceNumber:0

SS_IntegrityProtActivationTimeInfo:

rb_Identity:1
rrc_MessageSequenceNumber:0

SS_IntegrityProtActivationTimeInfo:

rb_Identity:3
rrc_MessageSequenceNumber:0

SS_IntegrityProtActivationTimeInfo:

rb_Identity:4
rrc_MessageSequenceNumber:0

#### CMAC Integrity Check Request

RRC MAC @ 00:00:36.070

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000001
Data:

[0]00 00 00 01
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:1 (RNC to UE)
Message Length (bits):192
Message:

[0]80 00 00 01 81 40 01 E0
[8]A0 40 1E 22 00 00 22 E0
[16]BE 82 24 46 68 94 34 40

#### CMAC Integrity Check Result

MAC RRC @ 00:00:36.070

Message Details:

Integrity Check Result:

MAC-I:00010011010010000100010001011010
Data:

[0]13 48 44 5A

#### CRLC_Integrity_Activate_CNF

LLA RRC @ 00:00:36.070

Cell ID: -1

Message Details:

CRLC_Integrity_Activate_CNF:

cellId:-1

#### RRC_DATA_REQ: mm:locationUpdatingAccept

NAS RRC @ 00:00:36.070

Cell ID: -1

Message Details:

LOCATIONUPDATINGACCEPT:

skipIndicator: 0000

mMProtocolDiscriminator: 0101

msgType: 00000010

locAreaId:

plmn: 00F110

lac: 0001

mobileId:

iei: 00010111

iel: 05

iDigit1: 1111

oddEvenInd: 0

typeOfId: 100

otherDigits: 11223344

followOnProceed: 10100001

cTSPerm: 10100010

equivalentPLMN: Omitted

#### RLC_AM_DATA_REQ:downlinkDirectTransfer

RRC RLC @ 00:00:36.070

Channel No: 3 Name: DCCH

Message Details:

Opt1: 0

Opt2: 0

DL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode: 00010011010010000100010001011010

rrc_MessageSequenceNumber: 1

message:

downlinkDirectTransfer:

r3:

downlinkDirectTransfer_r3:

rrc_TransactionIdentifier: 0

cn_DomainIdentity: cs_domain_CN_DomainIdentity [enum=0]

nas_Message: 050200F11000011705F411223344A1A2

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]89 A4 22 2D 09 40 01 E0
[8]A0 40 1E 22 00 00 22 E0
[16]BE 82 24 46 68 94 34 40

#### MAC_DATA_REQ

RLC MAC @ 00:00:36.180

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 43

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 18 89 A4 22 2D 09 40
[8]01 E0 A0 40 1E 22 00 00
[16]22 E0

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:3
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]89 A4 22 2D 09 40 01 E0
[8]A0 40 1E 22 00 00 22 E0

#### MAC_DATA_REQ

RLC MAC @ 00:00:36.180

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 43

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 25 11 FE BE 82 24 46
[8]68 94 34 40 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:4
Polling bit:1 (request a status report)
Length indicator 0 (octets):8
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (8 octets):

[0]BE 82 24 46 68 94 34 40
Padding associated with length indicator 1 (6 octets):

[0]00 00 00 00 00 00

#### PHY_DATA_REQ

MAC PHY @ 00:00:36.180

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 43

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 01 88 9A 42 22 D0 94
[8]00 1E 0A 04 01 E2 20 00
[16]02 2E 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 18 89 A4 22 2D 09 40
[8]01 E0 A0 40 1E 22 00 00
[16]22 E0

#### PHY_DATA_REQ

MAC PHY @ 00:00:36.190

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 44

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 02 51 1F EB E8 22 44
[8]66 89 43 44 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 25 11 FE BE 82 24 46
[8]68 94 34 40 00 00 00 00
[16]00 00

#### MAC_DATA_REQ

RLC MAC @ 00:00:36.380

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 63

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 25 11 FE BE 82 24 46
[8]68 94 34 40 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:4
Polling bit:1 (request a status report)
Length indicator 0 (octets):8
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (8 octets):

[0]BE 82 24 46 68 94 34 40
Padding associated with length indicator 1 (6 octets):

[0]00 00 00 00 00 00

#### PHY_DATA_REQ

MAC PHY @ 00:00:36.380

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 63

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 02 51 1F EB E8 22 44
[8]66 89 43 44 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 25 11 FE BE 82 24 46
[8]68 94 34 40 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:00:36.430

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 48

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 05 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 50 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### MAC_DATA_IND

MAC RLC @ 00:00:36.430

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 48

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 50 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:5

#### PHY_DATA_IND

PHY MAC @ 00:00:36.440

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 49

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 02 51 5F EA 4D 81 B8
[8]D8 EC 00 08 2C D8 05 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 25 15 FE A4 D8 1B 8D
[8]8E C0 00 82 CD 80 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:00:36.440

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 49

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 25 15 FE A4 D8 1B 8D
[8]8E C0 00 82 CD 80 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:4
Polling bit:1 (request a status report)
Length indicator 0 (octets):10
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (10 octets):

[0]A4 D8 1B 8D 8E C0 00 82
[8]CD 80
Padding associated with length indicator 1 (4 octets):

[0]55 55 55 55

#### RLC_AM_DATA_IND: uplinkDirectTransfer

RLC RRC @ 00:00:36.450

Channel No: 3 Name: DCCH

Message Details:

UL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode: 01001001101100000011011100011011

rrc_MessageSequenceNumber: 1

message:

uplinkDirectTransfer:

cn_DomainIdentity: cs_domain_CN_DomainIdentity [enum=0]

nas_Message: 059B

measuredResultsOnRACH: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]A4 D8 1B 8D 8E C0 00 82
[8]CD 80

#### RRC_DATA_IND: mm:tmsiReallocationComplete

RRC NAS @ 00:00:36.450

Cell ID: -1

Message Details:

TMSIREALLOCATIONCOMPLETE:

skipIndicator: 0000

mMProtocolDiscriminator: 0101

msgType: 10011011

#### MAC_DATA_REQ

RLC MAC @ 00:00:36.450

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 70

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 50 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:5

#### CMAC Integrity Check Request

RRC MAC @ 00:00:36.460

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000001
Data:

[0]00 00 00 01
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:0 (UE to RNC)
Message Length (bits):80
Message:

[0]80 00 00 01 86 C0 00 82
[8]CD 80

#### CMAC Integrity Check Result

MAC RRC @ 00:00:36.460

Message Details:

Integrity Check Result:

MAC-I:01001001101100000011011100011011
Data:

[0]49 B0 37 1B

#### PHY_DATA_REQ

MAC PHY @ 00:00:36.450

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 70

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 05 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 50 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:00:36.630

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 68

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 05 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 50 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### MAC_DATA_IND

MAC RLC @ 00:00:36.630

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 68

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 50 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:5

#### PHY_DATA_IND

PHY MAC @ 00:00:36.640

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 69

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 02 51 5F EA 4D 81 B8
[8]D8 EC 00 08 2C D8 05 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 25 15 FE A4 D8 1B 8D
[8]8E C0 00 82 CD 80 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:00:36.640

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 69

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 25 15 FE A4 D8 1B 8D
[8]8E C0 00 82 CD 80 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:4
Polling bit:1 (request a status report)
Length indicator 0 (octets):10
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (10 octets):

[0]A4 D8 1B 8D 8E C0 00 82
[8]CD 80
Padding associated with length indicator 1 (4 octets):

[0]55 55 55 55

#### MAC_DATA_REQ

RLC MAC @ 00:00:36.650

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 90

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 50 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:5

#### PHY_DATA_REQ

MAC PHY @ 00:00:36.650

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 90

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 05 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 50 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### CMAC Integrity Check Request

RRC MAC @ 00:00:37.470

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000001
Data:

[0]00 00 00 01
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:1 (RNC to UE)
Message Length (bits):56
Message:

[0]80 00 00 00 83 C8 00

#### CMAC Integrity Check Result

MAC RRC @ 00:00:37.470

Message Details:

Integrity Check Result:

MAC-I:11101100100111000001011111010011
Data:

[0]EC 9C 17 D3

#### RLC_UM_DATA_REQ

RRC LLA @ 00:00:37.470

Channel ID: Rb1
Cell ID: -1

Message Details:

RLC_UM_DATA_REQ:

cellId:-1

routingInfo:

rB_Identity:1

uM_message:

dL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode:00000000000000000000000000000000
rrc_MessageSequenceNumber:0

message: (DL_DCCH_MessageType)

rrcConnectionRelease:

r3:

rrcConnectionRelease_r3: (RRCConnectionRelease_r3_IEs)

rrc_TransactionIdentifier:0
n_308:1
releaseCause:normalEvent

rplmn_information: Omit

laterNonCriticalExtensions: Omit

specialLI:false

#### RLC_UM_DATA_REQ: rrcConnectionRelease

LLA RLC @ 00:00:37.470

Channel No: 1 Name: DCCH

Message Details:

DL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode: 11101100100111000001011111010011

rrc_MessageSequenceNumber: 1

message:

rrcConnectionRelease:

r3:

rrcConnectionRelease_r3:

rrc_TransactionIdentifier: 0

n_308: 1

releaseCause: normalEvent_ReleaseCause [enum=0]

rplmn_information: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]F6 4E 0B E9 8B C8 00

#### MAC_DATA_REQ

RLC MAC @ 00:00:37.510

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 176

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]01 0F FE F6 4E 0B E9 8B
[8]C8 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

Sequence number:0
Length indicator 0 (octets):7
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (7 octets):

[0]F6 4E 0B E9 8B C8 00
Padding associated with length indicator 1 (8 octets):

[0]00 00 00 00 00 00 00 00

#### PHY_DATA_REQ

MAC PHY @ 00:00:37.510

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 176

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]00 10 FF EF 64 E0 BE 98
[8]BC 80 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:0
MAC SDU (144 bits):

[0]01 0F FE F6 4E 0B E9 8B
[8]C8 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:00:37.750

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 180

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]00 10 DF EF BF 16 16 70
[8]C4 05 55 55 55 55 55 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:0
MAC SDU (144 bits):

[0]01 0D FE FB F1 61 67 0C
[8]40 55 55 55 55 55 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:00:37.750

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 180

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]01 0D FE FB F1 61 67 0C
[8]40 55 55 55 55 55 55 55
[16]55 55

RLC PDU (decoded):

Sequence number:0
Length indicator 0 (octets):6
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (6 octets):

[0]FB F1 61 67 0C 40
Padding associated with length indicator 1 (9 octets):

[0]55 55 55 55 55 55 55 55
[8]55

#### CMAC Integrity Check Request

RRC MAC @ 00:00:37.770

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000001
Data:

[0]00 00 00 01
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:0 (UE to RNC)
Message Length (bits):48
Message:

[0]80 00 00 00 84 40

#### RLC_UM_DATA_IND: rrcConnectionReleaseComplete

RLC LLA @ 00:00:37.770

Channel No: 1 Name: DCCH

Message Details:

UL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode: 11110111111000101100001011001110

rrc_MessageSequenceNumber: 1

message:

rrcConnectionReleaseComplete:

rrc_TransactionIdentifier: 0

errorIndication: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]FB F1 61 67 0C 40

#### CMAC Integrity Check Result

MAC RRC @ 00:00:37.770

Message Details:

Integrity Check Result:

MAC-I:11110111111000101100001011001110
Data:

[0]F7 E2 C2 CE

#### RLC_UM_DATA_IND

LLA RRC @ 00:00:37.770

Channel ID: Rb1
Cell ID: -1

Message Details:

RLC_UM_DATA_IND:

cellId:-1

routingInfo:

rB_Identity:1

integrityResult:

integrityUsed (IntegrityStatus):i_pass

uM_message:

uL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode:11110111111000101100001011001110
rrc_MessageSequenceNumber:1

message: (UL_DCCH_MessageType)

rrcConnectionReleaseComplete:

rrc_TransactionIdentifier:0

errorIndication: (FailureCauseWithProtErr) Omit

laterNonCriticalExtensions: Omit

#### PHY_DATA_IND

PHY MAC @ 00:00:37.900

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 195

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]00 30 DF ED CD 18 3E 01
[8]44 05 55 55 55 55 55 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:0
MAC SDU (144 bits):

[0]03 0D FE DC D1 83 E0 14
[8]40 55 55 55 55 55 55 55
[16]55 55

#### CMAC Integrity Check Request

RRC MAC @ 00:00:37.910

Category: Configuration

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000010
Data:

[0]00 00 00 02
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:0 (UE to RNC)
Message Length (bits):48
Message:

[0]80 00 00 00 84 40

#### RLC_UM_DATA_IND: rrcConnectionReleaseComplete

RLC LLA @ 00:00:37.910

Channel No: 1 Name: DCCH

Message Details:

UL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode: 10111001101000110000011111000000

rrc_MessageSequenceNumber: 2

message:

rrcConnectionReleaseComplete:

rrc_TransactionIdentifier: 0

errorIndication: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]DC D1 83 E0 14 40

#### CMAC Integrity Check Result

MAC RRC @ 00:00:37.910

Message Details:

Integrity Check Result:

MAC-I:10111001101000110000011111000000
Data:

[0]B9 A3 07 C0

#### MAC_DATA_IND

MAC RLC @ 00:00:37.900

BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 195

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]03 0D FE DC D1 83 E0 14
[8]40 55 55 55 55 55 55 55
[16]55 55

RLC PDU (decoded):

Sequence number:1
Length indicator 0 (octets):6
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (6 octets):

[0]DC D1 83 E0 14 40
Padding associated with length indicator 1 (9 octets):

[0]55 55 55 55 55 55 55 55
[8]55

#### RLC_UM_DATA_IND

LLA RRC @ 00:00:37.910

Channel ID: Rb1
Cell ID: -1

Message Details:

RLC_UM_DATA_IND:

cellId:-1

routingInfo:

rB_Identity:1

integrityResult:

integrityUsed (IntegrityStatus):i_pass

uM_message:

uL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode:10111001101000110000011111000000
rrc_MessageSequenceNumber:2

message: (UL_DCCH_MessageType)

rrcConnectionReleaseComplete:

rrc_TransactionIdentifier:0

errorIndication: (FailureCauseWithProtErr) Omit

laterNonCriticalExtensions: Omit

#### CRLC_Config_REQ

RRC LLA @ 00:00:37.910

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:1

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CPHY_OUTSYNC_IND

PHY RRC @ 00:00:37.970

BTS unit: 1:1
Channel No: 0 Name: U_DPCH
CFN: 222

Message Details:

#### CRLC UM Channel Release REQ

LLA RLC @ 00:00:37.990

BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 224

Message Details:

#### CRLC UM Channel Release CNF

RLC LLA @ 00:00:37.990

BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 224

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:00:38.020

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:1

#### CRLC_Config_REQ

RRC LLA @ 00:00:38.020

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:2

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC AM Channel Release REQ

LLA RLC @ 00:00:38.130

BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 238

Message Details:

#### CRLC AM Channel Release CNF

RLC LLA @ 00:00:38.130

BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 238

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:00:38.160

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:2

#### CRLC_Config_REQ

RRC LLA @ 00:00:38.160

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:3

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC AM Channel Release REQ

LLA RLC @ 00:00:38.310

BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 0

Message Details:

#### CRLC AM Channel Release CNF

RLC LLA @ 00:00:38.310

BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 0

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:00:38.330

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:3

#### CRLC_Config_REQ

RRC LLA @ 00:00:38.330

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:4

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC_Config_CNF

LLA RRC @ 00:00:38.360

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:4

#### CRLC_Config_REQ

RRC LLA @ 00:00:38.360

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:1

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode)

dl_UM_RLC_Mode:

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):136

dl_RLCModeInfo: (UL_RLC_Mode)

ul_UM_RLC_Mode:

transmissionRLC_Discard:

timerBasedNoExplicit (NoExplicitDiscard):dt100

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity):1
dLlogicalChannelIdentity (LogicalChannelIdentity):1
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC AM Channel Release REQ

LLA RLC @ 00:00:38.360

BTS unit: 1:1
Channel No: 4 Name: DCCH
CFN: 5

Message Details:

#### CRLC AM Channel Release CNF

RLC LLA @ 00:00:38.360

BTS unit: 1:1
Channel No: 4 Name: DCCH
CFN: 5

Message Details:

#### CRLC UM Channel Establish REQ

LLA RLC @ 00:00:38.470

BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 16

Message Details:

Configuration Parameters:

PU Size In Bits:136

#### CRLC UM Channel Establish CNF

RLC LLA @ 00:00:38.470

BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 16

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:00:38.510

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:1

#### CRLC_Config_REQ

RRC LLA @ 00:00:38.510

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:2

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode)

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):128

dl_RLCModeInfo: (UL_RLC_Mode)

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity):2
dLlogicalChannelIdentity (LogicalChannelIdentity):2
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC AM Channel Establish REQ

LLA RLC @ 00:00:38.570

BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 26

Message Details:

Configuration Parameters:

PU Size In Bits:128

Timer Parameters:

Poll (ms):200
Poll Prohibit (ms):0
EPC (ms):0
Discard (ms):0
Poll Periodic (ms):0
Status Prohibit (ms):0
Status Periodic (ms):0
Reset (ms):500
MRW (ms):0

Protocol Parameters:

Max Dat:15
Poll PU:0
Poll SDU:1
Poll Window:99
Max Reset:1
Tx Window Size:32
Rx Window Size:32
Max MRW:0
SDU Discard Mode:No discard

Polling Triggers:

Last PU In Buffer:On
Last PU In Retransmission Buffer:On
Poll Timer:On
Every Poll-PU PU:Off
Every Poll-SDU SDU:On
Poll-Window Percent Of Transmission Buffer:On
Timer Based:Off

Status Triggers:

Missing PU:On
Timer Based:Off
EPC Mechanism:Off

#### CRLC AM Channel Establish CNF

RLC LLA @ 00:00:38.570

BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 26

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:00:38.580

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:2

#### CRLC_Config_REQ

RRC LLA @ 00:00:38.580

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:3

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode)

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):128

dl_RLCModeInfo: (UL_RLC_Mode)

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity):3
dLlogicalChannelIdentity (LogicalChannelIdentity):3
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC AM Channel Establish REQ

LLA RLC @ 00:00:38.630

BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 32

Message Details:

Configuration Parameters:

PU Size In Bits:128

Timer Parameters:

Poll (ms):200
Poll Prohibit (ms):0
EPC (ms):0
Discard (ms):0
Poll Periodic (ms):0
Status Prohibit (ms):0
Status Periodic (ms):0
Reset (ms):500
MRW (ms):0

Protocol Parameters:

Max Dat:15
Poll PU:0
Poll SDU:1
Poll Window:99
Max Reset:1
Tx Window Size:32
Rx Window Size:32
Max MRW:0
SDU Discard Mode:No discard

Polling Triggers:

Last PU In Buffer:On
Last PU In Retransmission Buffer:On
Poll Timer:On
Every Poll-PU PU:Off
Every Poll-SDU SDU:On
Poll-Window Percent Of Transmission Buffer:On
Timer Based:Off

Status Triggers:

Missing PU:On
Timer Based:Off
EPC Mechanism:Off

#### CRLC AM Channel Establish CNF

RLC LLA @ 00:00:38.630

BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 32

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:00:38.650

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:3

#### CRLC_Config_REQ

RRC LLA @ 00:00:38.650

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:4

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode)

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):128

dl_RLCModeInfo: (UL_RLC_Mode)

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity):4
dLlogicalChannelIdentity (LogicalChannelIdentity):4
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC AM Channel Establish REQ

LLA RLC @ 00:00:38.780

BTS unit: 1:1
Channel No: 4 Name: DCCH
CFN: 47

Message Details:

Configuration Parameters:

PU Size In Bits:128

Timer Parameters:

Poll (ms):200
Poll Prohibit (ms):0
EPC (ms):0
Discard (ms):0
Poll Periodic (ms):0
Status Prohibit (ms):0
Status Periodic (ms):0
Reset (ms):500
MRW (ms):0

Protocol Parameters:

Max Dat:15
Poll PU:0
Poll SDU:1
Poll Window:99
Max Reset:1
Tx Window Size:32
Rx Window Size:32
Max MRW:0
SDU Discard Mode:No discard

Polling Triggers:

Last PU In Buffer:On
Last PU In Retransmission Buffer:On
Poll Timer:On
Every Poll-PU PU:Off
Every Poll-SDU SDU:On
Poll-Window Percent Of Transmission Buffer:On
Timer Based:Off

Status Triggers:

Missing PU:On
Timer Based:Off
EPC Mechanism:Off

#### CRLC AM Channel Establish CNF

RLC LLA @ 00:00:38.780

BTS unit: 1:1
Channel No: 4 Name: DCCH
CFN: 47

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:00:38.790

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:4

#### AT_CmdReq

RRC LLA @ 00:00:39.800

Message Details:

AT_CmdReq:

cmd (IA5String):AT+CGATT=1<CR>
sMS_BlockMode (HEXSTRING):

Omit

#### AT_CmdCnf

LLA RRC @ 00:00:42.070

Message Details:

AT_CmdCnf:

result: Omit
resultString (IA5String):<CR><LF>OK<CR><LF>
sMS_BlockMode (HEXSTRING):

Omit

#### PHY_DATA_IND

PHY MAC @ 00:00:47.300

BTS unit: 1:1
Channel No: 0 Name: U_RACH
CFN: 111

Message Details:

TFI:0
TB set size:168
TB size:168
TB set (raw):

[0]08 44 48 8C D1 00 04 02
[8]00 02 C0 00 00 00 00 00
[16]00 00 00 00 00 00

TB set (decoded):

TB 0:

TCTF:0
MAC SDU (166 bits):

[0]21 11 22 33 44 00 10 08
[8]00 0B 00 00 00 00 00 00
[16]00 00 00 00 00

#### MAC_DATA_IND

MAC RLC @ 00:00:47.300

Category: Configuration
BTS unit: 1:1
Channel No: 0 Name: CCCH
CFN: 111

Message Details:

RLC PDU size (bits):166
RLC PDU (raw):

[0]21 11 22 33 44 00 10 08
[8]00 0B 00 00 00 00 00 00
[16]00 00 00 00 00

#### RLC_TR_DATA_IND: rrcConnectionRequest

RLC LLA @ 00:00:47.330

Channel No: 0 Name: CCCH

Message Details:

UL_CCCH_Message:

integrityCheckInfo: Omitted

message:

rrcConnectionRequest:

initialUE_Identity:

tmsi_and_LAI:

tmsi: 00010001001000100011001101000100

lai:

plmn_Identity:

mcc:

MCC.element: 0

MCC.element: 0

MCC.element: 1

mnc:

MNC.element: 0

MNC.element: 1

lac: 0000000000000001

establishmentCause: registration_EstablishmentCause [enum=12]

protocolErrorIndicator: noError_ProtocolErrorIndicator [enum=0]

measuredResultsOnRACH: Omitted

v3d0NonCriticalExtensions: Omitted

Layer 3 SDU:

[0]21 11 22 33 44 00 10 08
[8]00 0B 00 00 00 00 00 00
[16]00 00 00 00 00

#### RLC_TR_DATA_IND

LLA RRC @ 00:00:47.330

Channel ID: Rb0
Cell ID: 0

Message Details:

RLC_TR_DATA_IND:

cellId:0

routingInfo:

rB_Identity:0

tM_message:

uL_CCCH_Message:

integrityCheckInfo: Omit

message: (UL_CCCH_MessageType)

rrcConnectionRequest:

initialUE_Identity:

tmsi_and_LAI: (TMSI_and_LAI_GSM_MAP)

tmsi (TMSI_GSM_MAP):00010001001000100011001101000100

lai:

plmn_Identity:

mcc:

Digit:0
Digit:0
Digit:1

mnc:

Digit:0
Digit:1

lac:0000000000000001

establishmentCause:registration
protocolErrorIndicator:noError

measuredResultsOnRACH: Omit

v3d0NonCriticalExtensions: Omit

#### RLC_UM_DATA_REQ

RRC LLA @ 00:00:47.330

Channel ID: Rb0
Cell ID: 0

Message Details:

RLC_UM_DATA_REQ:

cellId:0

routingInfo:

rB_Identity:0

uM_message:

dL_CCCH_Message:

integrityCheckInfo: Omit

message: (DL_CCCH_MessageType)

rrcConnectionSetup:

r3:

rrcConnectionSetup_r3: (RRCConnectionSetup_r3_IEs)

initialUE_Identity:

tmsi_and_LAI: (TMSI_and_LAI_GSM_MAP)

tmsi (TMSI_GSM_MAP):00010001001000100011001101000100

lai:

plmn_Identity:

mcc:

Digit:0
Digit:0
Digit:1

mnc:

Digit:0
Digit:1

lac:0000000000000001

rrc_TransactionIdentifier:0
activationTime: Omit

new_U_RNTI: (U_RNTI)

srnc_Identity:000000000001
s_RNTI:00000000000000000001

new_c_RNTI (C_RNTI): Omit
rrc_StateIndicator:cell_DCH
utran_DRX_CycleLengthCoeff (UTRAN_DRX_CycleLengthCoefficient):9

capabilityUpdateRequirement:

ue_RadioCapabilityFDDUpdateRequirement:true
ue_RadioCapabilityTDDUpdateRequirement:false

systemSpecificCapUpdateReqList:

SystemSpecificCapUpdateReq:gsm

srb_InformationSetupList: (SRB_InformationSetupList2)

SRB_InformationSetup:

rb_Identity: Omit

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_UM_RLC_Mode:

transmissionRLC_Discard: Omit

dl_RLC_Mode:

dl_UM_RLC_Mode:

rb_MappingInfo:

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

dch (TransportChannelIdentity):5

logicalChannelIdentity:1

rlc_SizeList:

configured:

mac_LogicalChannelPriority:1

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

dch (TransportChannelIdentity):10

logicalChannelIdentity:1

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

rach:

logicalChannelIdentity:1

rlc_SizeList:

explicitList: (RLC_SizeExplicitList)

RLC_SizeInfo:

rlc_SizeIndex:1

mac_LogicalChannelPriority:1

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

fach:

logicalChannelIdentity:1

SRB_InformationSetup:

rb_Identity: Omit

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

rb_MappingInfo:

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

dch (TransportChannelIdentity):5

logicalChannelIdentity:2

rlc_SizeList:

configured:

mac_LogicalChannelPriority:2

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

dch (TransportChannelIdentity):10

logicalChannelIdentity:2

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

rach:

logicalChannelIdentity:2

rlc_SizeList:

explicitList: (RLC_SizeExplicitList)

RLC_SizeInfo:

rlc_SizeIndex:1

mac_LogicalChannelPriority:2

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

fach:

logicalChannelIdentity:2

SRB_InformationSetup:

rb_Identity: Omit

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

rb_MappingInfo:

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

dch (TransportChannelIdentity):5

logicalChannelIdentity:3

rlc_SizeList:

configured:

mac_LogicalChannelPriority:3

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

dch (TransportChannelIdentity):10

logicalChannelIdentity:3

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

rach:

logicalChannelIdentity:3

rlc_SizeList:

explicitList: (RLC_SizeExplicitList)

RLC_SizeInfo:

rlc_SizeIndex:1

mac_LogicalChannelPriority:3

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

fach:

logicalChannelIdentity:3

SRB_InformationSetup:

rb_Identity: Omit

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

rb_MappingInfo:

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

dch (TransportChannelIdentity):5

logicalChannelIdentity:4

rlc_SizeList:

configured:

mac_LogicalChannelPriority:4

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

dch (TransportChannelIdentity):10

logicalChannelIdentity:4

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

rach:

logicalChannelIdentity:4

rlc_SizeList:

explicitList: (RLC_SizeExplicitList)

RLC_SizeInfo:

rlc_SizeIndex:1

mac_LogicalChannelPriority:4

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

fach:

logicalChannelIdentity:4

ul_CommonTransChInfo:

tfc_Subset: Omit

prach_TFCS: (TFCS) Omit

modeSpecificInfo:

fdd:

ul_TFCS: (TFCS)

normalTFCI_Signalling: (ExplicitTFCS_Configuration)

complete: (TFCS_ReconfAdd)

ctfcSize:

ctfc2Bit:

:

ctfc2:0

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc2:1

powerOffsetInformation:

gainFactorInformation:

signalledGainFactors:

modeSpecificInfo:

fdd:

gainFactorBetaC (GainFactor):11

gainFactorBetaD (GainFactor):15
referenceTFC_ID:0

powerOffsetPp_m: Omit

ul_AddReconfTransChInfoList:

UL_AddReconfTransChInformation:

ul_TransportChannelType (UL_TrCH_Type):dch
transportChannelIdentity:5

transportFormatSet:

dedicatedTransChTFS:

tti:

tti10: (DedicatedDynamicTF_InfoList)

DedicatedDynamicTF_Info:

rlc_Size:

bitMode: (BitModeRLC_SizeInfo)

sizeType2:

part1:2
part2: Omit

numberOfTbSizeList:

NumberOfTransportBlocks:

zero:

NumberOfTransportBlocks:

one:

logicalChannelList:

allSizes:

semistaticTF_Information:

channelCodingType:

convolutional (CodingRate):third

rateMatchingAttribute:192
crc_Size:crc16

dl_CommonTransChInfo:

sccpch_TFCS: (TFCS) Omit

modeSpecificInfo:

fdd:

dl_Parameters:

sameAsUL:

dl_AddReconfTransChInfoList:

DL_AddReconfTransChInformation:

dl_TransportChannelType (DL_TrCH_Type):dch
dl_transportChannelIdentity (TransportChannelIdentity):10

tfs_SignallingMode:

sameAsULTrCH: (UL_TransportChannelIdentity)

ul_TransportChannelType (UL_TrCH_Type):dch
ul_TransportChannelIdentity (TransportChannelIdentity):5

dch_QualityTarget: (QualityTarget)

bler_QualityValue:-20

dummy: (TM_SignallingInfo) Omit

frequencyInfo: Omit

maxAllowedUL_TX_Power: Omit

ul_ChannelRequirement:

ul_DPCH_Info:

ul_DPCH_PowerControlInfo:

fdd:

dpcch_PowerOffset:-40
pc_Preamble:1
sRB_delay:7

powerControlAlgorithm:

algorithm1 (TPC_StepSizeFDD):1

modeSpecificInfo:

fdd:

scramblingCodeType:longSC
scramblingCode (UL_ScramblingCode):0
numberOfDPDCH: Omit
spreadingFactor:sf64
tfci_Existence:true
numberOfFBI_Bits: Omit
puncturingLimit:pl1

dl_CommonInformation:

dl_DPCH_InfoCommon:

cfnHandling:

initialise:

cfntargetsfnframeoffset: Omit

modeSpecificInfo:

fdd:

dl_DPCH_PowerControlInfo:

modeSpecificInfo:

fdd:

dpc_Mode:singleTPC

powerOffsetPilot_pdpdch:0

dl_rate_matching_restriction: Omit

spreadingFactorAndPilot: (SF512_AndPilot)

sfd128 (PilotBits128):pb4

positionFixedOrFlexible:fixed
tfci_Existence:false

modeSpecificInfo:

fdd:

defaultDPCH_OffsetValue (DefaultDPCH_OffsetValueFDD):0

dpch_CompressedModeInfo: Omit

tx_DiversityMode:noDiversity

ssdt_Information: Omit

dl_InformationPerRL_List:

DL_InformationPerRL:

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode:100

pdsch_SHO_DCH_Info: Omit

pdsch_CodeMapping: Omit

dl_DPCH_InfoPerRL:

fdd:

pCPICH_UsageForChannelEst:mayBeUsed
dpch_FrameOffset:0

secondaryCPICH_Info: Omit

dl_ChannelisationCodeList:

DL_ChannelisationCode:

secondaryScramblingCode:1

sf_AndCodeNumber: (SF512_AndCodeNumber)

sf128:0

scramblingCodeChange:noCodeChange

tpc_CombinationIndex:0
ssdt_CellIdentity: Omit
closedLoopTimingAdjMode: Omit

sccpch_InfoforFACH: Omit

laterNonCriticalExtensions: Omit

specialLI:true

#### RLC_UM_DATA_REQ: rrcConnectionSetup

LLA RLC @ 00:00:47.330

Channel No: 1 Name: CCCH

Message Details:

DL_CCCH_Message:

integrityCheckInfo: Omitted

message:

rrcConnectionSetup:

r3:

rrcConnectionSetup_r3:

initialUE_Identity:

tmsi_and_LAI:

tmsi: 00010001001000100011001101000100

lai:

plmn_Identity:

mcc:

MCC.element: 0

MCC.element: 0

MCC.element: 1

mnc:

MNC.element: 0

MNC.element: 1

lac: 0000000000000001

rrc_TransactionIdentifier: 0

activationTime: Omitted

new_U_RNTI:

srnc_Identity: 000000000001

s_RNTI: 00000000000000000001

new_c_RNTI: Omitted

rrc_StateIndicator: cell_DCH_RRC_StateIndicator [enum=0]

utran_DRX_CycleLengthCoeff: 9

capabilityUpdateRequirement:

ue_RadioCapabilityFDDUpdateRequirement: 1

ue_RadioCapabilityTDDUpdateRequirement: 0

systemSpecificCapUpdateReqList:

SystemSpecificCapUpdateReqList.element: gsm_SystemSpecificCapUpdateReq [enum=0]

srb_InformationSetupList:

SRB_InformationSetupList2.element:

rb_Identity: Omitted

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_UM_RLC_Mode:

transmissionRLC_Discard: Omitted

dl_RLC_Mode:

dl_UM_RLC_Mode: NULL

rb_MappingInfo:

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

dch: 5

logicalChannelIdentity: 1

rlc_SizeList:

configured: NULL

mac_LogicalChannelPriority: 1

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

dch: 10

logicalChannelIdentity: 1

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

rach: NULL

logicalChannelIdentity: 1

rlc_SizeList:

explicitList:

RLC_SizeExplicitList.element:

rlc_SizeIndex: 1

mac_LogicalChannelPriority: 1

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

fach: NULL

logicalChannelIdentity: 1

SRB_InformationSetupList2.element:

rb_Identity: Omitted

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard: dat15_MaxDAT [enum=10]

transmissionWindowSize: tw32_TransmissionWindowSize [enum=3]

timerRST: tr500_TimerRST [enum=9]

max_RST: rst1_MaxRST [enum=0]

pollingInfo:

timerPollProhibit: tpp200_TimerPollProhibit [enum=19]

timerPoll: tp200_TimerPoll [enum=19]

poll_PDU: Omitted

poll_SDU: sdu1_Poll_SDU [enum=0]

lastTransmissionPDU_Poll: 1

lastRetransmissionPDU_Poll: 1

pollWindow: pw99_PollWindow [enum=7]

timerPollPeriodic: Omitted

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery: 1

receivingWindowSize: rw32_ReceivingWindowSize [enum=3]

dl_RLC_StatusInfo:

timerStatusProhibit: tsp200_TimerStatusProhibit [enum=19]

timerEPC: Omitted

missingPDU_Indicator: 1

timerStatusPeriodic: Omitted

rb_MappingInfo:

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

dch: 5

logicalChannelIdentity: 2

rlc_SizeList:

configured: NULL

mac_LogicalChannelPriority: 2

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

dch: 10

logicalChannelIdentity: 2

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

rach: NULL

logicalChannelIdentity: 2

rlc_SizeList:

explicitList:

RLC_SizeExplicitList.element:

rlc_SizeIndex: 1

mac_LogicalChannelPriority: 2

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

fach: NULL

logicalChannelIdentity: 2

SRB_InformationSetupList2.element:

rb_Identity: Omitted

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard: dat15_MaxDAT [enum=10]

transmissionWindowSize: tw32_TransmissionWindowSize [enum=3]

timerRST: tr500_TimerRST [enum=9]

max_RST: rst1_MaxRST [enum=0]

pollingInfo:

timerPollProhibit: tpp200_TimerPollProhibit [enum=19]

timerPoll: tp200_TimerPoll [enum=19]

poll_PDU: Omitted

poll_SDU: sdu1_Poll_SDU [enum=0]

lastTransmissionPDU_Poll: 1

lastRetransmissionPDU_Poll: 1

pollWindow: pw99_PollWindow [enum=7]

timerPollPeriodic: Omitted

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery: 1

receivingWindowSize: rw32_ReceivingWindowSize [enum=3]

dl_RLC_StatusInfo:

timerStatusProhibit: tsp200_TimerStatusProhibit [enum=19]

timerEPC: Omitted

missingPDU_Indicator: 1

timerStatusPeriodic: Omitted

rb_MappingInfo:

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

dch: 5

logicalChannelIdentity: 3

rlc_SizeList:

configured: NULL

mac_LogicalChannelPriority: 3

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

dch: 10

logicalChannelIdentity: 3

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

rach: NULL

logicalChannelIdentity: 3

rlc_SizeList:

explicitList:

RLC_SizeExplicitList.element:

rlc_SizeIndex: 1

mac_LogicalChannelPriority: 3

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

fach: NULL

logicalChannelIdentity: 3

SRB_InformationSetupList2.element:

rb_Identity: Omitted

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard: dat15_MaxDAT [enum=10]

transmissionWindowSize: tw32_TransmissionWindowSize [enum=3]

timerRST: tr500_TimerRST [enum=9]

max_RST: rst1_MaxRST [enum=0]

pollingInfo:

timerPollProhibit: tpp200_TimerPollProhibit [enum=19]

timerPoll: tp200_TimerPoll [enum=19]

poll_PDU: Omitted

poll_SDU: sdu1_Poll_SDU [enum=0]

lastTransmissionPDU_Poll: 1

lastRetransmissionPDU_Poll: 1

pollWindow: pw99_PollWindow [enum=7]

timerPollPeriodic: Omitted

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery: 1

receivingWindowSize: rw32_ReceivingWindowSize [enum=3]

dl_RLC_StatusInfo:

timerStatusProhibit: tsp200_TimerStatusProhibit [enum=19]

timerEPC: Omitted

missingPDU_Indicator: 1

timerStatusPeriodic: Omitted

rb_MappingInfo:

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

dch: 5

logicalChannelIdentity: 4

rlc_SizeList:

configured: NULL

mac_LogicalChannelPriority: 4

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

dch: 10

logicalChannelIdentity: 4

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

rach: NULL

logicalChannelIdentity: 4

rlc_SizeList:

explicitList:

RLC_SizeExplicitList.element:

rlc_SizeIndex: 1

mac_LogicalChannelPriority: 4

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

fach: NULL

logicalChannelIdentity: 4

ul_CommonTransChInfo:

tfc_Subset: Omitted

prach_TFCS: Omitted

modeSpecificInfo:

fdd:

ul_TFCS:

normalTFCI_Signalling:

complete:

ctfcSize:

ctfc2Bit:

ctfc2Bit.noName:

ctfc2: 0

powerOffsetInformation:

gainFactorInformation:

computedGainFactors: 0

powerOffsetPp_m: Omitted

ctfc2Bit.noName:

ctfc2: 1

powerOffsetInformation:

gainFactorInformation:

signalledGainFactors:

modeSpecificInfo:

fdd:

gainFactorBetaC: 11

gainFactorBetaD: 15

referenceTFC_ID: 0

powerOffsetPp_m: Omitted

ul_AddReconfTransChInfoList:

UL_AddReconfTransChInfoList.element:

ul_TransportChannelType: dch_UL_TrCH_Type [enum=0]

transportChannelIdentity: 5

transportFormatSet:

dedicatedTransChTFS:

tti:

tti10:

DedicatedDynamicTF_InfoList.element:

rlc_Size:

bitMode:

sizeType2:

part1: 2

part2: Omitted

numberOfTbSizeList:

numberOfTbSizeList.element:

zero: NULL

numberOfTbSizeList.element:

one: NULL

logicalChannelList:

allSizes: NULL

semistaticTF_Information:

channelCodingType:

convolutional: third_CodingRate [enum=1]

rateMatchingAttribute: 192

crc_Size: crc16_CRC_Size [enum=3]

dl_CommonTransChInfo:

sccpch_TFCS: Omitted

modeSpecificInfo:

fdd:

dl_Parameters:

sameAsUL: NULL

dl_AddReconfTransChInfoList:

DL_AddReconfTransChInfoList.element:

dl_TransportChannelType: dch_DL_TrCH_Type [enum=0]

dl_transportChannelIdentity: 10

tfs_SignallingMode:

sameAsULTrCH:

ul_TransportChannelType: dch_UL_TrCH_Type [enum=0]

ul_TransportChannelIdentity: 5

dch_QualityTarget:

bler_QualityValue: -20

dummy: Omitted

frequencyInfo: Omitted

maxAllowedUL_TX_Power: Omitted

ul_ChannelRequirement:

ul_DPCH_Info:

ul_DPCH_PowerControlInfo:

fdd:

dpcch_PowerOffset: -40

pc_Preamble: 1

sRB_delay: 7

powerControlAlgorithm:

algorithm1: 1

modeSpecificInfo:

fdd:

scramblingCodeType: longSC_ScramblingCodeType [enum=1]

scramblingCode: 0

numberOfDPDCH: Default

spreadingFactor: sf64_SpreadingFactor [enum=4]

tfci_Existence: 1

numberOfFBI_Bits: Omitted

puncturingLimit: pl1_PuncturingLimit [enum=15]

dl_CommonInformation:

dl_DPCH_InfoCommon:

cfnHandling:

initialise:

cfntargetsfnframeoffset: Omitted

modeSpecificInfo:

fdd:

dl_DPCH_PowerControlInfo:

modeSpecificInfo:

fdd:

dpc_Mode: singleTPC_DPC_Mode [enum=0]

powerOffsetPilot_pdpdch: 0

dl_rate_matching_restriction: Omitted

spreadingFactorAndPilot:

sfd128: pb4_PilotBits128 [enum=0]

positionFixedOrFlexible: fixed_PositionFixedOrFlexible [enum=0]

tfci_Existence: 0

modeSpecificInfo:

fdd:

defaultDPCH_OffsetValue: 0

dpch_CompressedModeInfo: Omitted

tx_DiversityMode: noDiversity_TX_DiversityMode [enum=0]

ssdt_Information: Omitted

dl_InformationPerRL_List:

DL_InformationPerRL_List.element:

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode: 100

pdsch_SHO_DCH_Info: Omitted

pdsch_CodeMapping: Omitted

dl_DPCH_InfoPerRL:

fdd:

pCPICH_UsageForChannelEst: mayBeUsed_PCPICH_UsageForChannelEst [enum=0]

dpch_FrameOffset: 0

secondaryCPICH_Info: Omitted

dl_ChannelisationCodeList:

DL_ChannelisationCodeList.element:

secondaryScramblingCode: 1

sf_AndCodeNumber:

sf128: 0

scramblingCodeChange: noCodeChange_ScramblingCodeChange [enum=1]

tpc_CombinationIndex: 0

ssdt_CellIdentity: Omitted

closedLoopTimingAdjMode: Omitted

sccpch_InfoforFACH: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]30 E7 22 24 46 68 80 02
[8]01 00 01 00 04 00 00 4D
[16]82 69 3A 10 10 89 0D 42
[24]00 02 81 9E 8E 46 C9 A6
[32]7C 9C 4E 74 20 A5 12 3A
[40]8C 00 15 13 3D 1C 8D 93
[48]4C F9 38 9C E8 42 52 24
[56]B5 28 00 4A 46 7A 39 1B
[64]26 99 F2 71 39 D0 86 B4
[72]49 EA 70 00 D4 C8 00 06
[80]25 2B F0 02 00 08 82 23
[88]BF 66 08 98 95 A5 47 A2
[96]00 00 01 3F 90 0A 14 00
[104]02 06 40 00 0C 28 08

#### MAC_DATA_REQ

RLC MAC @ 00:00:47.430

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: CCCH
CFN: 144

Message Details:

RLC PDU size (bits):160
RLC PDU (raw):

[0]0D F8 30 E7 22 24 46 68
[8]80 02 01 00 01 00 04 00
[16]00 4D 82 69

RLC PDU (decoded):

Sequence number:6
Length indicator 0 (octets):124 (the first data octet in this RLC PDU is the first octet of a RLC SDU)
Segment associated with length indicator 0 (0 octets):

Last segment, not associated with any length indicators (18 octets):

[0]30 E7 22 24 46 68 80 02
[8]01 00 01 00 04 00 00 4D
[16]82 69

#### MAC_DATA_REQ

RLC MAC @ 00:00:47.430

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: CCCH
CFN: 144

Message Details:

RLC PDU size (bits):160
RLC PDU (raw):

[0]0E 3A 10 10 89 0D 42 00
[8]02 81 9E 8E 46 C9 A6 7C
[16]9C 4E 74 20

RLC PDU (decoded):

Sequence number:7
Last segment, not associated with any length indicators (19 octets):

[0]3A 10 10 89 0D 42 00 02
[8]81 9E 8E 46 C9 A6 7C 9C
[16]4E 74 20

#### MAC_DATA_REQ

RLC MAC @ 00:00:47.430

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: CCCH
CFN: 144

Message Details:

RLC PDU size (bits):160
RLC PDU (raw):

[0]10 A5 12 3A 8C 00 15 13
[8]3D 1C 8D 93 4C F9 38 9C
[16]E8 42 52 24

RLC PDU (decoded):

Sequence number:8
Last segment, not associated with any length indicators (19 octets):

[0]A5 12 3A 8C 00 15 13 3D
[8]1C 8D 93 4C F9 38 9C E8
[16]42 52 24

#### MAC_DATA_REQ

RLC MAC @ 00:00:47.430

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: CCCH
CFN: 144

Message Details:

RLC PDU size (bits):160
RLC PDU (raw):

[0]12 B5 28 00 4A 46 7A 39
[8]1B 26 99 F2 71 39 D0 86
[16]B4 49 EA 70

RLC PDU (decoded):

Sequence number:9
Last segment, not associated with any length indicators (19 octets):

[0]B5 28 00 4A 46 7A 39 1B
[8]26 99 F2 71 39 D0 86 B4
[16]49 EA 70

#### MAC_DATA_REQ

RLC MAC @ 00:00:47.430

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: CCCH
CFN: 144

Message Details:

RLC PDU size (bits):160
RLC PDU (raw):

[0]14 00 D4 C8 00 06 25 2B
[8]F0 02 00 08 82 23 BF 66
[16]08 98 95 A5

RLC PDU (decoded):

Sequence number:10
Last segment, not associated with any length indicators (19 octets):

[0]00 D4 C8 00 06 25 2B F0
[8]02 00 08 82 23 BF 66 08
[16]98 95 A5

#### MAC_DATA_REQ

RLC MAC @ 00:00:47.430

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: CCCH
CFN: 144

Message Details:

RLC PDU size (bits):160
RLC PDU (raw):

[0]17 23 FE 47 A2 00 00 01
[8]3F 90 0A 14 00 02 06 40
[16]00 0C 28 08

RLC PDU (decoded):

Sequence number:11
Length indicator 0 (octets):17
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (17 octets):

[0]47 A2 00 00 01 3F 90 0A
[8]14 00 02 06 40 00 0C 28
[16]08
Padding associated with length indicator 1 (0 octets):

#### PHY_DATA_REQ

MAC PHY @ 00:00:47.430

BTS unit: 1:1
Channel No: 0 Name: FACH
CFN: 144

Message Details:

TFI:2
TB set size:336
TB size:168
TB set (raw, each TB word aligned):

[0]40 0D F8 30 E7 22 24 46
[8]68 80 02 01 00 01 00 04
[16]00 00 4D 82 69 00 40 0E
[24]3A 10 10 89 0D 42 00 02
[32]81 9E 8E 46 C9 A6 7C 9C
[40]4E 74 20 00

TB set (decoded):

TB 0:

TCTF:64
MAC SDU (160 bits):

[0]0D F8 30 E7 22 24 46 68
[8]80 02 01 00 01 00 04 00
[16]00 4D 82 69

TB 1:

TCTF:64
MAC SDU (160 bits):

[0]0E 3A 10 10 89 0D 42 00
[8]02 81 9E 8E 46 C9 A6 7C
[16]9C 4E 74 20

#### PHY_DATA_REQ

MAC PHY @ 00:00:47.440

BTS unit: 1:1
Channel No: 0 Name: FACH
CFN: 145

Message Details:

TFI:2
TB set size:336
TB size:168
TB set (raw, each TB word aligned):

[0]40 10 A5 12 3A 8C 00 15
[8]13 3D 1C 8D 93 4C F9 38
[16]9C E8 42 52 24 00 40 12
[24]B5 28 00 4A 46 7A 39 1B
[32]26 99 F2 71 39 D0 86 B4
[40]49 EA 70 00

TB set (decoded):

TB 0:

TCTF:64
MAC SDU (160 bits):

[0]10 A5 12 3A 8C 00 15 13
[8]3D 1C 8D 93 4C F9 38 9C
[16]E8 42 52 24

TB 1:

TCTF:64
MAC SDU (160 bits):

[0]12 B5 28 00 4A 46 7A 39
[8]1B 26 99 F2 71 39 D0 86
[16]B4 49 EA 70

#### PHY_DATA_REQ

MAC PHY @ 00:00:47.450

BTS unit: 1:1
Channel No: 0 Name: FACH
CFN: 146

Message Details:

TFI:2
TB set size:336
TB size:168
TB set (raw, each TB word aligned):

[0]40 14 00 D4 C8 00 06 25
[8]2B F0 02 00 08 82 23 BF
[16]66 08 98 95 A5 00 40 17
[24]23 FE 47 A2 00 00 01 3F
[32]90 0A 14 00 02 06 40 00
[40]0C 28 08 00

TB set (decoded):

TB 0:

TCTF:64
MAC SDU (160 bits):

[0]14 00 D4 C8 00 06 25 2B
[8]F0 02 00 08 82 23 BF 66
[16]08 98 95 A5

TB 1:

TCTF:64
MAC SDU (160 bits):

[0]17 23 FE 47 A2 00 00 01
[8]3F 90 0A 14 00 02 06 40
[16]00 0C 28 08

#### CPHY_SYNC_IND

PHY RRC @ 00:00:47.730

BTS unit: 1:1
Channel No: 0 Name: U_DPCH
CFN: 174

Message Details:

#### PHY_DATA_IND

PHY MAC @ 00:00:47.900

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 171

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 00 04 A0 C0 00 08 00
[8]00 5E 23 41 A2 09 09 8C
[16]D0 8C 50 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 00 4A 0C 00 00 80 00
[8]05 E2 34 1A 20 90 98 CD
[16]08 C5

#### MAC_DATA_IND

MAC RLC @ 00:00:47.900

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 171

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 00 4A 0C 00 00 80 00
[8]05 E2 34 1A 20 90 98 CD
[16]08 C5

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:0
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]4A 0C 00 00 80 00 05 E2
[8]34 1A 20 90 98 CD 08 C5

#### PHY_DATA_IND

PHY MAC @ 00:00:47.910

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 172

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 00 D1 5F E9 26 04 10
[8]00 10 00 23 1F 1F 05 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 0D 15 FE 92 60 41 00
[8]01 00 02 31 F1 F0 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:00:47.910

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 172

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 0D 15 FE 92 60 41 00
[8]01 00 02 31 F1 F0 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:1
Polling bit:1 (request a status report)
Length indicator 0 (octets):10
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (10 octets):

[0]92 60 41 00 01 00 02 31
[8]F1 F0
Padding associated with length indicator 1 (4 octets):

[0]55 55 55 55

#### MAC_DATA_REQ

RLC MAC @ 00:00:47.920

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 193

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 20 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:2

#### PHY_DATA_REQ

MAC PHY @ 00:00:47.920

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 193

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]10 20 02 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]02 00 20 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:00:47.920

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 173

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 00 01 58 0D 10 10 04
[8]00 81 72 A0 09 83 81 02
[16]FA 09 10 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 00 15 80 D1 01 00 40
[8]08 17 2A 00 98 38 10 2F
[16]A0 91

#### MAC_DATA_IND

MAC RLC @ 00:00:47.920

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 173

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 00 15 80 D1 01 00 40
[8]08 17 2A 00 98 38 10 2F
[16]A0 91

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:0
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]15 80 D1 01 00 40 08 17
[8]2A 00 98 38 10 2F A0 91

#### PHY_DATA_IND

PHY MAC @ 00:00:47.930

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 174

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 00 8A 2B 3C 00 78 88
[8]00 00 82 85 0A 79 C1 19
[16]A6 01 90 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 08 A2 B3 C0 07 88 80
[8]00 08 28 50 A7 9C 11 9A
[16]60 19

#### MAC_DATA_IND

MAC RLC @ 00:00:47.930

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 174

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 08 A2 B3 C0 07 88 80
[8]00 08 28 50 A7 9C 11 9A
[16]60 19

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:1
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]A2 B3 C0 07 88 80 00 08
[8]28 50 A7 9C 11 9A 60 19

#### PHY_DATA_IND

PHY MAC @ 00:00:47.940

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 175

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 01 51 3F E3 1E 50 30
[8]0B 8B 20 00 04 05 55 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 15 13 FE 31 E5 03 00
[8]B8 B2 00 00 40 55 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:00:47.940

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 175

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 15 13 FE 31 E5 03 00
[8]B8 B2 00 00 40 55 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:2
Polling bit:1 (request a status report)
Length indicator 0 (octets):9
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (9 octets):

[0]31 E5 03 00 B8 B2 00 00
[8]40
Padding associated with length indicator 1 (5 octets):

[0]55 55 55 55 55

#### RLC_AM_DATA_IND: rrcConnectionSetupComplete

RLC LLA @ 00:00:47.940

Channel No: 2 Name: DCCH

Message Details:

UL_DCCH_Message:

integrityCheckInfo: Omitted

message:

rrcConnectionSetupComplete:

rrc_TransactionIdentifier: 0

startList:

STARTList.element:

cn_DomainIdentity: ps_domain_CN_DomainIdentity [enum=1]

start_Value: 00000000000000000010

STARTList.element:

cn_DomainIdentity: cs_domain_CN_DomainIdentity [enum=0]

start_Value: 00000000000000000010

ue_RadioAccessCapability:

accessStratumReleaseIndicator: r99_AccessStratumReleaseIndicator [enum=0]

pdcp_Capability:

losslessSRNS_RelocationSupport: 1

supportForRfc2507:

supported: by8192_MaxHcContextSpace [enum=4]

rlc_Capability:

totalRLC_AM_BufferSize: kb50_TotalRLC_AM_BufferSize [enum=2]

maximumRLC_WindowSize: mws2047_MaximumRLC_WindowSize [enum=0]

maximumAM_EntityNumber: am6_MaximumAM_EntityNumberRLC_Cap [enum=3]

transportChannelCapability:

dl_TransChCapability:

maxNoBitsReceived: b5120_MaxNoBits [enum=4]

maxConvCodeBitsReceived: b1280_MaxNoBits [enum=1]

turboDecodingSupport:

supported: b5120_MaxNoBits [enum=4]

maxSimultaneousTransChs: e8_MaxSimultaneousTransChsDL [enum=1]

maxSimultaneousCCTrCH_Count: 1

maxReceivedTransportBlocks: tb16_MaxTransportBlocksDL [enum=2]

maxNumberOfTFC: tfc96_MaxNumberOfTFC_DL [enum=4]

maxNumberOfTF: tf64_MaxNumberOfTF [enum=1]

ul_TransChCapability:

maxNoBitsTransmitted: b3840_MaxNoBits [enum=3]

maxConvCodeBitsTransmitted: b1280_MaxNoBits [enum=1]

turboEncodingSupport:

supported: b3840_MaxNoBits [enum=3]

maxSimultaneousTransChs: e8_MaxSimultaneousTransChsUL [enum=2]

modeSpecificInfo:

fdd: NULL

maxTransmittedBlocks: tb8_MaxTransportBlocksUL [enum=2]

maxNumberOfTFC: tfc32_MaxNumberOfTFC_UL [enum=3]

maxNumberOfTF: tf32_MaxNumberOfTF [enum=0]

rf_Capability:

fddRF_Capability:

ue_PowerClass: 4

txRxFrequencySeparation: mhz190_TxRxFrequencySeparation [enum=0]

tddRF_Capability: Omitted

physicalChannelCapability:

fddPhysChCapability:

downlinkPhysChCapability:

maxNoDPCH_PDSCH_Codes: 3

maxNoPhysChBitsReceived: b9600_MaxNoPhysChBitsReceived [enum=6]

supportForSF_512: 0

supportOfPDSCH: 0

simultaneousSCCPCH_DPCH_Reception:

notSupported: NULL

uplinkPhysChCapability:

maxNoDPDCH_BitsTransmitted: b2400_MaxNoDPDCH_BitsTransmitted [enum=2]

supportOfPCPCH: 0

tddPhysChCapability: Omitted

ue_MultiModeRAT_Capability:

multiRAT_CapabilityList:

supportOfGSM: 0

supportOfMulticarrier: 0

multiModeCapability: fdd_MultiModeCapability [enum=1]

securityCapability:

cipheringAlgorithmCap: 0000000000000001

integrityProtectionAlgorithmCap: 0000000000000010

ue_positioning_Capability:

standaloneLocMethodsSupported: 0

ue_BasedOTDOA_Supported: 0

networkAssistedGPS_Supported: noNetworkAssistedGPS_NetworkAssistedGPS_Supported [enum=3]

supportForUE_GPS_TimingOfCellFrames: 0

supportForIPDL: 0

measurementCapability:

downlinkCompressedMode:

fdd_Measurements: 1

tdd_Measurements: Omitted

gsm_Measurements:

gsm900: 1

dcs1800: 1

gsm1900: 0

multiCarrierMeasurements: 0

uplinkCompressedMode:

fdd_Measurements: 1

tdd_Measurements: Omitted

gsm_Measurements:

gsm900: 1

dcs1800: 1

gsm1900: 0

multiCarrierMeasurements: 0

ue_RATSpecificCapability: Omitted

v370NonCriticalExtensions: Omitted

Layer 3 SDU:

[0]4A 0C 00 00 80 00 05 E2
[8]34 1A 20 90 98 CD 08 C5
[16]92 60 41 00 01 00 02 31
[24]F1 F0

#### MAC_DATA_REQ

RLC MAC @ 00:00:47.950

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 196

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:3

#### PHY_DATA_REQ

MAC PHY @ 00:00:47.950

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 196

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 03 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### RLC_AM_DATA_IND

LLA RRC @ 00:00:47.960

Channel ID: Rb2
Cell ID: -1

Message Details:

RLC_AM_DATA_IND:

cellId:-1

routingInfo:

rB_Identity:2

integrityResult:

integrityUsed (IntegrityStatus):i_pass

aM_message:

uL_DCCH_Message:

integrityCheckInfo: Omit

message: (UL_DCCH_MessageType)

rrcConnectionSetupComplete:

rrc_TransactionIdentifier:0

startList:

STARTSingle:

cn_DomainIdentity:ps_domain
start_Value:00000000000000000010

STARTSingle:

cn_DomainIdentity:cs_domain
start_Value:00000000000000000010

ue_RadioAccessCapability:

accessStratumReleaseIndicator:r99

pdcp_Capability:

losslessSRNS_RelocationSupport:true

supportForRfc2507:

supported (MaxHcContextSpace):by8192

rlc_Capability:

totalRLC_AM_BufferSize:kb50
maximumRLC_WindowSize:mws2047
maximumAM_EntityNumber (MaximumAM_EntityNumberRLC_Cap):am6

transportChannelCapability:

dl_TransChCapability:

maxNoBitsReceived (MaxNoBits):b5120
maxConvCodeBitsReceived (MaxNoBits):b1280

turboDecodingSupport: (TurboSupport)

supported (MaxNoBits):b5120

maxSimultaneousTransChs (MaxSimultaneousTransChsDL):e8
maxSimultaneousCCTrCH_Count:1
maxReceivedTransportBlocks (MaxTransportBlocksDL):tb16
maxNumberOfTFC (MaxNumberOfTFC_DL):tfc96
maxNumberOfTF:tf64

ul_TransChCapability:

maxNoBitsTransmitted (MaxNoBits):b3840
maxConvCodeBitsTransmitted (MaxNoBits):b1280

turboEncodingSupport: (TurboSupport)

supported (MaxNoBits):b3840

maxSimultaneousTransChs (MaxSimultaneousTransChsUL):e8

modeSpecificInfo:

fdd:

maxTransmittedBlocks (MaxTransportBlocksUL):tb8
maxNumberOfTFC (MaxNumberOfTFC_UL):tfc32
maxNumberOfTF:tf32

rf_Capability:

fddRF_Capability:

ue_PowerClass:4
txRxFrequencySeparation:mhz190

tddRF_Capability: Omit

physicalChannelCapability:

fddPhysChCapability:

downlinkPhysChCapability: (DL_PhysChCapabilityFDD)

maxNoDPCH_PDSCH_Codes:3
maxNoPhysChBitsReceived:b9600
supportForSF_512:false
supportOfPDSCH:false

simultaneousSCCPCH_DPCH_Reception:

notSupported:

uplinkPhysChCapability: (UL_PhysChCapabilityFDD)

maxNoDPDCH_BitsTransmitted:b2400
supportOfPCPCH:false

tddPhysChCapability: Omit

ue_MultiModeRAT_Capability:

multiRAT_CapabilityList: (MultiRAT_Capability)

supportOfGSM:false
supportOfMulticarrier:false

multiModeCapability:fdd

securityCapability:

cipheringAlgorithmCap:0000000000000001
integrityProtectionAlgorithmCap:0000000000000010

ue_positioning_Capability:

standaloneLocMethodsSupported:false
ue_BasedOTDOA_Supported:false
networkAssistedGPS_Supported:noNetworkAssistedGPS
supportForUE_GPS_TimingOfCellFrames:false
supportForIPDL:false

measurementCapability:

downlinkCompressedMode: (CompressedModeMeasCapability)

fdd_Measurements:true
tdd_Measurements: Omit

gsm_Measurements:

gsm900:true
dcs1800:true
gsm1900:false

multiCarrierMeasurements:false

uplinkCompressedMode: (CompressedModeMeasCapability)

fdd_Measurements:true
tdd_Measurements: Omit

gsm_Measurements:

gsm900:true
dcs1800:true
gsm1900:false

multiCarrierMeasurements:false

ue_RATSpecificCapability: (InterRAT_UE_RadioAccessCapabilityList) Omit

v370NonCriticalExtensions: Omit

#### RLC_AM_DATA_IND: initialDirectTransfer

RLC RRC @ 00:00:47.950

Channel No: 3 Name: DCCH

Message Details:

UL_DCCH_Message:

integrityCheckInfo: Omitted

message:

initialDirectTransfer:

cn_DomainIdentity: ps_domain_CN_DomainIdentity [enum=1]

intraDomainNasNodeSelector:

version:

release99:

cn_Type:

gsm_Map_IDNNS:

routingbasis:

localPTMSI:

routingparameter: 0011010001

enteredparameter: 0

nas_Message: 080102E54013070205F41234567800F1100001050A14F382334C03263CA0601716

measuredResultsOnRACH: Omitted

v3a0NonCriticalExtensions:

initialDirectTransfer_v3a0ext:

start_Value: 00000000000000000010

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]15 80 D1 01 00 40 08 17
[8]2A 00 98 38 10 2F A0 91
[16]A2 B3 C0 07 88 80 00 08
[24]28 50 A7 9C 11 9A 60 19
[32]31 E5 03 00 B8 B2 00 00
[40]40

#### RRC_DATA_IND: gmm:attachRequest

RRC NAS @ 00:00:47.950

Cell ID: -1

Message Details:

ATTACHREQUEST:

skipIndicator: 0000

gMMProtocolDiscriminator: 1000

msgType: 00000001

msNetworkCap:

iel: 02

value: E540

gprsCiphKeySeqNo:

spare1: 0

keySeq: 001

attachType:

for: 0

type: 011

drxParameter:

splitPGcycleCode: 00000111

cnDRXcoef: 0000

splitOnCCCH: 0

nonDRXtimer: 010

ptmsiORimsi:

iel: 05

iDigit1: 1111

oddEvenInd: 0

typeOfId: 100

otherDigits: 12345678

oldRAI:

plmn: 00F110

lac: 0001

rac: 05

msRadioAccessCap:

iel: 0A

value: 14F382334C03263CA060

oldPTMSI_Signature: Omitted

readyTimer:

iei: 00010111

unit: 000

value: 10110

tmsiStatus: Omitted

#### RRC_DATA_REQ: gmm:authenticationAndCipheringRequest

NAS RRC @ 00:00:47.970

Cell ID: -1

Message Details:

AUTHENTICATIONANDCIPHERINGREQUEST:

skipIndicator: 0000

gMMProtocolDiscriminator: 1000

msgType: 00010010

imeisvReq:

spare1: 0

value: 000

ciphAlgorithm:

spare1: 0

algorithm: 001

acRefNo:

value: 0011

forceToStandby:

spare: 0

value: 000

authRand:

iei: 00100001

randValue: 01010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101

gprsCiphKeySeqNo:

iei: 1000

spare1: 0

keySeq: 000

aUTN:

iei: 00101000

iel: 10

aUTN: 01100110000100010000000000110011001000101101110100000000000000000101010101000100011101110110011000010001000000000011001100100010

#### RLC_AM_DATA_REQ:downlinkDirectTransfer

RRC RLC @ 00:00:47.990

Channel No: 3 Name: DCCH

Message Details:

Opt1: 0

Opt2: 0

DL_DCCH_Message:

integrityCheckInfo: Omitted

message:

downlinkDirectTransfer:

r3:

downlinkDirectTransfer_r3:

rrc_TransactionIdentifier: 0

cn_DomainIdentity: ps_domain_CN_DomainIdentity [enum=1]

nas_Message: 0812013021555555555555555555555555555555558028106611003322DD00005544776611003322

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]14 20 4E 10 24 02 60 42
[8]AA AA AA AA AA AA AA AA
[16]AA AA AA AA AA AA AA AB
[24]00 50 20 CC 22 00 66 45
[32]BA 00 00 AA 88 EE CC 22
[40]00 66 44

#### MAC_DATA_REQ

RLC MAC @ 00:00:48.070

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 208

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 00 14 20 4E 10 24 02
[8]60 42 AA AA AA AA AA AA
[16]AA AA

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:0
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]14 20 4E 10 24 02 60 42
[8]AA AA AA AA AA AA AA AA

#### MAC_DATA_REQ

RLC MAC @ 00:00:48.070

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 208

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 08 AA AA AA AA AA AA
[8]AA AB 00 50 20 CC 22 00
[16]66 45

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:1
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]AA AA AA AA AA AA AA AB
[8]00 50 20 CC 22 00 66 45

#### MAC_DATA_REQ

RLC MAC @ 00:00:48.070

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 208

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 15 17 FE BA 00 00 AA
[8]88 EE CC 22 00 66 44 00
[16]00 00

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:2
Polling bit:1 (request a status report)
Length indicator 0 (octets):11
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (11 octets):

[0]BA 00 00 AA 88 EE CC 22
[8]00 66 44
Padding associated with length indicator 1 (3 octets):

[0]00 00 00

#### PHY_DATA_REQ

MAC PHY @ 00:00:48.070

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 208

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 00 01 42 04 E1 02 40
[8]26 04 2A AA AA AA AA AA
[16]AA AA A0 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 00 14 20 4E 10 24 02
[8]60 42 AA AA AA AA AA AA
[16]AA AA

#### PHY_DATA_REQ

MAC PHY @ 00:00:48.080

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 209

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 00 8A AA AA AA AA AA
[8]AA AA B0 05 02 0C C2 20
[16]06 64 50 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 08 AA AA AA AA AA AA
[8]AA AB 00 50 20 CC 22 00
[16]66 45

#### PHY_DATA_REQ

MAC PHY @ 00:00:48.090

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 210

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 01 51 7F EB A0 00 0A
[8]A8 8E EC C2 20 06 64 40
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 15 17 FE BA 00 00 AA
[8]88 EE CC 22 00 66 44 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:00:48.110

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 192

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 00 D1 5F E9 26 04 10
[8]00 10 00 23 1F 1F 05 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 0D 15 FE 92 60 41 00
[8]01 00 02 31 F1 F0 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:00:48.110

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 192

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 0D 15 FE 92 60 41 00
[8]01 00 02 31 F1 F0 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:1
Polling bit:1 (request a status report)
Length indicator 0 (octets):10
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (10 octets):

[0]92 60 41 00 01 00 02 31
[8]F1 F0
Padding associated with length indicator 1 (4 octets):

[0]55 55 55 55

#### MAC_DATA_REQ

RLC MAC @ 00:00:48.120

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 213

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 20 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:2

#### PHY_DATA_REQ

MAC PHY @ 00:00:48.120

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 213

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]10 20 02 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]02 00 20 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:00:48.140

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 195

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 01 51 3F E3 1E 50 30
[8]0B 8B 20 00 04 05 55 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 15 13 FE 31 E5 03 00
[8]B8 B2 00 00 40 55 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:00:48.140

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 195

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 15 13 FE 31 E5 03 00
[8]B8 B2 00 00 40 55 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:2
Polling bit:1 (request a status report)
Length indicator 0 (octets):9
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (9 octets):

[0]31 E5 03 00 B8 B2 00 00
[8]40
Padding associated with length indicator 1 (5 octets):

[0]55 55 55 55 55

#### MAC_DATA_REQ

RLC MAC @ 00:00:48.150

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 216

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:3

#### PHY_DATA_REQ

MAC PHY @ 00:00:48.150

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 216

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 03 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### MAC_DATA_REQ

RLC MAC @ 00:00:48.270

Category: Configuration
BTS unit: 1:
Channel No: 3 Name: DCCH
CFN: 228

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 15 17 FE BA 00 00 AA
[8]88 EE CC 22 00 66 44 00
[16]00 00

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:2
Polling bit:1 (request a status report)
Length indicator 0 (octets):11
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (11 octets):

[0]BA 00 00 AA 88 EE CC 22
[8]00 66 44
Padding associated with length indicator 1 (3 octets):

[0]00 00 00

#### PHY_DATA_REQ

MAC PHY @ 00:00:48.270

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 228

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 01 51 7F EB A0 00 0A
[8]A8 8E EC C2 20 06 64 40
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 15 17 FE BA 00 00 AA
[8]88 EE CC 22 00 66 44 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:00:48.330

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 214

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 03 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### MAC_DATA_IND

MAC RLC @ 00:00:48.330

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 214

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:3

#### PHY_DATA_IND

PHY MAC @ 00:00:48.470

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 228

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 01 86 C8 0A 84 09 81
[8]91 2A A2 3B B3 14 86 08
[16]80 19 90 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 18 6C 80 A8 40 98 19
[8]12 AA 23 BB 31 48 60 88
[16]01 99

#### MAC_DATA_IND

MAC RLC @ 00:00:48.470

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 228

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 18 6C 80 A8 40 98 19
[8]12 AA 23 BB 31 48 60 88
[16]01 99

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:3
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]6C 80 A8 40 98 19 12 AA
[8]23 BB 31 48 60 88 01 99

#### PHY_DATA_IND

PHY MAC @ 00:00:48.480

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 229

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 02 51 3F E1 6E E6 7F
[8]F7 4C C4 5D D5 05 55 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 25 13 FE 16 EE 67 FF
[8]74 CC 45 DD 50 55 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:00:48.480

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 229

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 25 13 FE 16 EE 67 FF
[8]74 CC 45 DD 50 55 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:4
Polling bit:1 (request a status report)
Length indicator 0 (octets):9
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (9 octets):

[0]16 EE 67 FF 74 CC 45 DD
[8]50
Padding associated with length indicator 1 (5 octets):

[0]55 55 55 55 55

#### RLC_AM_DATA_IND: uplinkDirectTransfer

RLC RRC @ 00:00:48.490

Channel No: 3 Name: DCCH

Message Details:

UL_DCCH_Message:

integrityCheckInfo: Omitted

message:

uplinkDirectTransfer:

cn_DomainIdentity: ps_domain_CN_DomainIdentity [enum=1]

nas_Message: 0813032255447766290C11003322DDCCFFEE9988BBAA

measuredResultsOnRACH: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]6C 80 A8 40 98 19 12 AA
[8]23 BB 31 48 60 88 01 99
[16]16 EE 67 FF 74 CC 45 DD
[24]50

#### RRC_DATA_IND: gmm:authenticationAndCipheringResponse

RRC NAS @ 00:00:48.490

Cell ID: -1

Message Details:

AUTHENTICATIONANDCIPHERINGRESPONSE:

skipIndicator: 0000

gMMProtocolDiscriminator: 1000

msgType: 00010011

spare4: 0000

acRefNo:

value: 0011

authRsp:

iei: 00100010

value: 01010101010001000111011101100110

imeisv: Omitted

authRspExt:

iei: 00101001

iel: 0C

rES: 000100010000000000110011001000101101110111001100111111111110111010011001100010001011101110101010

#### MAC_DATA_REQ

RLC MAC @ 00:00:48.490

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 250

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 50 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:5

#### PHY_DATA_REQ

MAC PHY @ 00:00:48.490

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 250

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 05 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 50 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### CRLC_SecurityMode_Config_REQ

RRC LLA @ 00:00:48.510

Cell ID: -1

Message Details:

CRLC_SecurityMode_Config_REQ:

cellId:-1

rlcSecurityInfo: (SecurityInfo)

cn_DomainIdentity:ps_domain
startValue (START_Value):00000000000000000000
cipheringKey: Omit
integrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
gsmCipheringKey: Omit

#### CRLC_SecurityMode_Config_REQ

RRC RLC @ 00:00:48.510

Message Details:

cellIdentity: 1

rlcSecurityInfo:

cn_DomainIdentity: ps_domain_CN_DomainIdentity

startValue: 00000000000000000000

cipheringKey: Omitted

integrityKey: 01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100

#### CRLC_SecurityMode_Config_CNF

LLA RRC @ 00:00:48.520

Cell ID: -1

Message Details:

CRLC_SecurityMode_Config_CNF:

cellId:-1

#### CRLC_SetRRC_MessageSN_REQ

RRC LLA @ 00:00:48.520

Channel ID: Rb0
Cell ID: 0

Message Details:

CRLC_SetRRC_MessageSN_REQ:

cellId:0

routingInfo:

rB_Identity:0

count_I_LSB_UL (RRC_SequenceNumber): Omit
count_I_LSB_DL (RRC_SequenceNumber):0

#### PHY_DATA_IND

PHY MAC @ 00:00:48.530

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 234

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 03 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### MAC_DATA_IND

MAC RLC @ 00:00:48.530

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 234

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:3

#### CRLC_SetRRC_MessageSN_CNF

LLA RRC @ 00:00:48.540

Channel ID: Rb0
Cell ID: 0

Message Details:

CRLC_SetRRC_MessageSN_CNF:

cellId:0

routingInfo:

rB_Identity:0

#### CRLC_SetRRC_MessageSN_REQ

RRC LLA @ 00:00:48.540

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_REQ:

cellId:-1

routingInfo:

rB_Identity:1

count_I_LSB_UL (RRC_SequenceNumber): Omit
count_I_LSB_DL (RRC_SequenceNumber):0

#### CRLC_SetRRC_MessageSN_CNF

LLA RRC @ 00:00:48.550

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_CNF:

cellId:-1

routingInfo:

rB_Identity:1

#### CRLC_SetRRC_MessageSN_REQ

RRC LLA @ 00:00:48.550

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_REQ:

cellId:-1

routingInfo:

rB_Identity:2

count_I_LSB_UL (RRC_SequenceNumber): Omit
count_I_LSB_DL (RRC_SequenceNumber):0

#### CRLC_SetRRC_MessageSN_CNF

LLA RRC @ 00:00:48.570

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_CNF:

cellId:-1

routingInfo:

rB_Identity:2

#### CRLC_SetRRC_MessageSN_REQ

RRC LLA @ 00:00:48.570

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_REQ:

cellId:-1

routingInfo:

rB_Identity:3

count_I_LSB_UL (RRC_SequenceNumber): Omit
count_I_LSB_DL (RRC_SequenceNumber):0

#### CRLC_SetRRC_MessageSN_CNF

LLA RRC @ 00:00:48.580

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_CNF:

cellId:-1

routingInfo:

rB_Identity:3

#### CRLC_SetRRC_MessageSN_REQ

RRC LLA @ 00:00:48.580

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_REQ:

cellId:-1

routingInfo:

rB_Identity:4

count_I_LSB_UL (RRC_SequenceNumber): Omit
count_I_LSB_DL (RRC_SequenceNumber):0

#### CRLC_SetRRC_MessageSN_CNF

LLA RRC @ 00:00:48.600

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_CNF:

cellId:-1

routingInfo:

rB_Identity:4

#### CRLC_Integrity_Activate_REQ

RRC LLA @ 00:00:48.600

Cell ID: -1

Message Details:

CRLC_Integrity_Activate_REQ:

cellId:-1
cn_DomainIdentity:ps_domain

integrityActivationInfo:

integrityProtectionModeInfo:

integrityProtectionModeCommand:

startIntegrityProtection:

integrityProtInitNumber:00001111000011110000111100001111

integrityProtectionAlgorithm:uia1

#### CRLC_Integrity_Activate_REQ

RRC RLC @ 00:00:48.600

Message Details:

cellIdentity: 1

integrityActivationInfo:

integrityProtectionModeInfo:

integrityProtectionModeCommand:

startIntegrityProtection:

integrityProtInitNumber: 00001111000011110000111100001111

#### CRLC_Integrity_Activate_CNF

LLA RRC @ 00:00:48.610

Cell ID: -1

Message Details:

CRLC_Integrity_Activate_CNF:

cellId:-1

#### CRLC_Integrity_Activate_REQ

RRC LLA @ 00:00:48.610

Cell ID: -1

Message Details:

CRLC_Integrity_Activate_REQ:

cellId:-1
cn_DomainIdentity:ps_domain

integrityActivationInfo:

ul_IntegProtActivationInfo: (IntegrityProtActivationInfoList)

SS_IntegrityProtActivationTimeInfo:

rb_Identity:2
rrc_MessageSequenceNumber:0

#### CMAC Integrity Check Request

RRC MAC @ 00:00:48.630

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000001
Data:

[0]00 00 00 01
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:1 (RNC to UE)
Message Length (bits):120
Message:

[0]80 00 00 01 04 04 00 00
[8]80 01 41 E1 E1 E1 F0

#### CMAC Integrity Check Result

MAC RRC @ 00:00:48.630

Message Details:

Integrity Check Result:

MAC-I:00101001110000010111010101011011
Data:

[0]29 C1 75 5B

#### CRLC_Integrity_Activate_CNF

LLA RRC @ 00:00:48.630

Cell ID: -1

Message Details:

CRLC_Integrity_Activate_CNF:

cellId:-1

#### RLC_AM_DATA_REQ

RRC LLA @ 00:00:48.630

Channel ID: Rb2
Cell ID: -1

Message Details:

RLC_AM_DATA_REQ:

cellId:-1

routingInfo:

rB_Identity:2

confirmationRequest: (AmConfirmationRequest)

noConfirmationRequest:

aM_message:

dL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode:00000000000000000000000000000000
rrc_MessageSequenceNumber:0

message: (DL_DCCH_MessageType)

securityModeCommand:

r3:

securityModeCommand_r3: (SecurityModeCommand_r3_IEs)

rrc_TransactionIdentifier:0

securityCapability:

cipheringAlgorithmCap:0000000000000001
integrityProtectionAlgorithmCap:0000000000000010

cipheringModeInfo: Omit

integrityProtectionModeInfo:

integrityProtectionModeCommand:

startIntegrityProtection:

integrityProtInitNumber:00001111000011110000111100001111

integrityProtectionAlgorithm:uia1

cn_DomainIdentity:ps_domain

ue_SystemSpecificSecurityCap: (InterRAT_UE_SecurityCapList) Omit

laterNonCriticalExtensions: Omit

#### RLC_AM_DATA_REQ: securityModeCommand

LLA RLC @ 00:00:48.630

Channel No: 2 Name: DCCH

Message Details:

DL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode: 00101001110000010111010101011011

rrc_MessageSequenceNumber: 1

message:

securityModeCommand:

r3:

securityModeCommand_r3:

rrc_TransactionIdentifier: 0

securityCapability:

cipheringAlgorithmCap: 0000000000000001

integrityProtectionAlgorithmCap: 0000000000000010

cipheringModeInfo: Omitted

integrityProtectionModeInfo:

integrityProtectionModeCommand:

startIntegrityProtection:

integrityProtInitNumber: 00001111000011110000111100001111

integrityProtectionAlgorithm: uia1_IntegrityProtectionAlgorithm [enum=0]

cn_DomainIdentity: ps_domain_CN_DomainIdentity [enum=1]

ue_SystemSpecificSecurityCap: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]94 E0 BA AD 8C 04 00 00
[8]80 01 41 E1 E1 E1 F0

#### PHY_DATA_IND

PHY MAC @ 00:00:48.690

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 250

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 02 51 3F E1 6E E6 7F
[8]F7 4C C4 5D D5 05 55 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 25 13 FE 16 EE 67 FF
[8]74 CC 45 DD 50 55 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:00:48.690

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 250

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 25 13 FE 16 EE 67 FF
[8]74 CC 45 DD 50 55 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:4
Polling bit:1 (request a status report)
Length indicator 0 (octets):9
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (9 octets):

[0]16 EE 67 FF 74 CC 45 DD
[8]50
Padding associated with length indicator 1 (5 octets):

[0]55 55 55 55 55

#### MAC_DATA_REQ

RLC MAC @ 00:00:48.700

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 15

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 50 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:5

#### PHY_DATA_REQ

MAC PHY @ 00:00:48.700

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 15

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 05 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 50 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### MAC_DATA_REQ

RLC MAC @ 00:00:48.710

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 16

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 05 1E 94 E0 BA AD 8C
[8]04 00 00 80 01 41 E1 E1
[16]E1 F0

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:0
Polling bit:1 (request a status report)
Length indicator 0 (octets):15
Segment associated with length indicator 0 (15 octets):

[0]94 E0 BA AD 8C 04 00 00
[8]80 01 41 E1 E1 E1 F0

#### PHY_DATA_REQ

MAC PHY @ 00:00:48.710

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 16

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 00 51 E9 4E 0B AA D8
[8]C0 40 00 08 00 14 1E 1E
[16]1E 1F 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 05 1E 94 E0 BA AD 8C
[8]04 00 00 80 01 41 E1 E1
[16]E1 F0

#### MAC_DATA_REQ

RLC MAC @ 00:00:48.910

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 36

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 05 1E 94 E0 BA AD 8C
[8]04 00 00 80 01 41 E1 E1
[16]E1 F0

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:0
Polling bit:1 (request a status report)
Length indicator 0 (octets):15
Segment associated with length indicator 0 (15 octets):

[0]94 E0 BA AD 8C 04 00 00
[8]80 01 41 E1 E1 E1 F0

#### PHY_DATA_REQ

MAC PHY @ 00:00:48.910

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 36

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 00 51 E9 4E 0B AA D8
[8]C0 40 00 08 00 14 1E 1E
[16]1E 1F 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 05 1E 94 E0 BA AD 8C
[8]04 00 00 80 01 41 E1 E1
[16]E1 F0

#### PHY_DATA_IND

PHY MAC @ 00:00:48.950

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 20

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]10 20 01 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]02 00 10 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### MAC_DATA_IND

MAC RLC @ 00:00:48.950

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 20

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 10 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:1

#### PHY_DATA_IND

PHY MAC @ 00:00:48.960

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 21

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 01 51 3F EC 59 1B E7
[8]10 D2 10 00 00 05 55 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 15 13 FE C5 91 BE 71
[8]0D 21 00 00 00 55 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:00:48.960

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 21

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 15 13 FE C5 91 BE 71
[8]0D 21 00 00 00 55 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:2
Polling bit:1 (request a status report)
Length indicator 0 (octets):9
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (9 octets):

[0]C5 91 BE 71 0D 21 00 00
[8]00
Padding associated with length indicator 1 (5 octets):

[0]55 55 55 55 55

#### MAC_DATA_REQ

RLC MAC @ 00:00:48.970

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 42

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:3

#### PHY_DATA_REQ

MAC PHY @ 00:00:48.970

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 42

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]10 20 03 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### CMAC Integrity Check Request

RRC MAC @ 00:00:48.990

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000001
Data:

[0]00 00 00 01
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:0 (UE to RNC)
Message Length (bits):72
Message:

[0]80 00 00 01 05 21 00 00
[8]00

#### RLC_AM_DATA_IND: securityModeComplete

RLC LLA @ 00:00:48.990

Channel No: 2 Name: DCCH

Message Details:

UL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode: 10001011001000110111110011100010

rrc_MessageSequenceNumber: 1

message:

securityModeComplete:

rrc_TransactionIdentifier: 0

ul_IntegProtActivationInfo:

rrc_MessageSequenceNumberList:

RRC_MessageSequenceNumberList.element: 0

RRC_MessageSequenceNumberList.element: 0

RRC_MessageSequenceNumberList.element: 0

RRC_MessageSequenceNumberList.element: 0

RRC_MessageSequenceNumberList.element: 0

rb_UL_CiphActivationTimeInfo: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]C5 91 BE 71 0D 21 00 00
[8]00

#### CMAC Integrity Check Result

MAC RRC @ 00:00:48.990

Message Details:

Integrity Check Result:

MAC-I:10001011001000110111110011100010
Data:

[0]8B 23 7C E2

#### RLC_AM_DATA_IND

LLA RRC @ 00:00:48.990

Channel ID: Rb2
Cell ID: -1

Message Details:

RLC_AM_DATA_IND:

cellId:-1

routingInfo:

rB_Identity:2

integrityResult:

integrityUsed (IntegrityStatus):i_pass

aM_message:

uL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode:10001011001000110111110011100010
rrc_MessageSequenceNumber:1

message: (UL_DCCH_MessageType)

securityModeComplete:

rrc_TransactionIdentifier:0

ul_IntegProtActivationInfo: (IntegrityProtActivationInfo)

rrc_MessageSequenceNumberList:

RRC_MessageSequenceNumber:0
RRC_MessageSequenceNumber:0
RRC_MessageSequenceNumber:0
RRC_MessageSequenceNumber:0
RRC_MessageSequenceNumber:0

rb_UL_CiphActivationTimeInfo: (RB_ActivationTimeInfoList) Omit

laterNonCriticalExtensions: Omit

#### CRLC_Integrity_Activate_REQ

RRC LLA @ 00:00:48.990

Cell ID: -1

Message Details:

CRLC_Integrity_Activate_REQ:

cellId:-1
cn_DomainIdentity:ps_domain

integrityActivationInfo:

ul_IntegProtActivationInfo: (IntegrityProtActivationInfoList)

SS_IntegrityProtActivationTimeInfo:

rb_Identity:0
rrc_MessageSequenceNumber:0

SS_IntegrityProtActivationTimeInfo:

rb_Identity:1
rrc_MessageSequenceNumber:0

SS_IntegrityProtActivationTimeInfo:

rb_Identity:3
rrc_MessageSequenceNumber:0

SS_IntegrityProtActivationTimeInfo:

rb_Identity:4
rrc_MessageSequenceNumber:0

#### CMAC Integrity Check Request

RRC MAC @ 00:00:49.010

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000001
Data:

[0]00 00 00 01
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:1 (RNC to UE)
Message Length (bits):296
Message:

[0]80 00 00 01 81 42 03 81
[8]00 40 7C 00 80 1E 22 00
[16]00 20 A3 35 62 46 83 00
[24]BE 82 46 8A CF 04 60 BE
[32]82 24 46 68 80

#### CMAC Integrity Check Result

MAC RRC @ 00:00:49.010

Message Details:

Integrity Check Result:

MAC-I:10100000000110000010111001100001
Data:

[0]A0 18 2E 61

#### CRLC_Integrity_Activate_CNF

LLA RRC @ 00:00:49.010

Cell ID: -1

Message Details:

CRLC_Integrity_Activate_CNF:

cellId:-1

#### RRC_DATA_REQ: gmm:attachAccept

NAS RRC @ 00:00:49.010

Cell ID: -1

Message Details:

ATTACHACCEPT:

skipIndicator: 0000

gMMProtocolDiscriminator: 1000

msgType: 00000010

forceToStandby:

spare: 0

value: 000

attachResult:

spare: 0

result: 011

periodicRAupdateTimer:

unit: 111

value: 00000

spare: 0000

radioPrioSMS:

spare: 0

value: 100

rai:

plmn: 00F110

lac: 0001

rac: 05

ptmsiSignature:

iei: 00011001

value: AB1234

negReadyTimer: Omitted

allocatedPTMSI:

iei: 00011000

iel: 05

iDigit1: 1111

oddEvenInd: 0

typeOfId: 100

otherDigits: 12345678

msIdentity:

iei: 00100011

iel: 05

iDigit1: 1111

oddEvenInd: 0

typeOfId: 100

otherDigits: 11223344

gmmCause: Omitted

t3302Value: Omitted

cellNotification: Omitted

equivalentPLMN: Omitted

#### RLC_AM_DATA_REQ:downlinkDirectTransfer

RRC RLC @ 00:00:49.010

Channel No: 3 Name: DCCH

Message Details:

Opt1: 0

Opt2: 0

DL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode: 10100000000110000010111001100001

rrc_MessageSequenceNumber: 1

message:

downlinkDirectTransfer:

r3:

downlinkDirectTransfer_r3:

rrc_TransactionIdentifier: 0

cn_DomainIdentity: ps_domain_CN_DomainIdentity [enum=1]

nas_Message: 080203E00400F11000010519AB12341805F4123456782305F411223344

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]D0 0C 17 30 89 42 03 81
[8]00 40 7C 00 80 1E 22 00
[16]00 20 A3 35 62 46 83 00
[24]BE 82 46 8A CF 04 60 BE
[32]82 24 46 68 80

#### MAC_DATA_REQ

RLC MAC @ 00:00:49.030

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 48

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 18 D0 0C 17 30 89 42
[8]03 81 00 40 7C 00 80 1E
[16]22 00

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:3
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]D0 0C 17 30 89 42 03 81
[8]00 40 7C 00 80 1E 22 00

#### MAC_DATA_REQ

RLC MAC @ 00:00:49.030

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 48

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 20 00 20 A3 35 62 46
[8]83 00 BE 82 46 8A CF 04
[16]60 BE

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:4
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]00 20 A3 35 62 46 83 00
[8]BE 82 46 8A CF 04 60 BE

#### MAC_DATA_REQ

RLC MAC @ 00:00:49.030

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 48

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 2D 0B FE 82 24 46 68
[8]80 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:5
Polling bit:1 (request a status report)
Length indicator 0 (octets):5
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (5 octets):

[0]82 24 46 68 80
Padding associated with length indicator 1 (9 octets):

[0]00 00 00 00 00 00 00 00
[8]00

#### PHY_DATA_REQ

MAC PHY @ 00:00:49.030

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 48

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 01 8D 00 C1 73 08 94
[8]20 38 10 04 07 C0 08 01
[16]E2 20 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 18 D0 0C 17 30 89 42
[8]03 81 00 40 7C 00 80 1E
[16]22 00

#### PHY_DATA_REQ

MAC PHY @ 00:00:49.040

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 49

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 02 00 02 0A 33 56 24
[8]68 30 0B E8 24 68 AC F0
[16]46 0B E0 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 20 00 20 A3 35 62 46
[8]83 00 BE 82 46 8A CF 04
[16]60 BE

#### PHY_DATA_REQ

MAC PHY @ 00:00:49.050

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 50

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 02 D0 BF E8 22 44 66
[8]88 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 2D 0B FE 82 24 46 68
[8]80 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:00:49.150

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 40

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]10 20 01 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]02 00 10 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### MAC_DATA_IND

MAC RLC @ 00:00:49.150

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 40

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 10 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:1

#### PHY_DATA_IND

PHY MAC @ 00:00:49.160

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 41

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 01 51 3F EC 59 1B E7
[8]10 D2 10 00 00 05 55 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 15 13 FE C5 91 BE 71
[8]0D 21 00 00 00 55 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:00:49.160

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 41

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 15 13 FE C5 91 BE 71
[8]0D 21 00 00 00 55 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:2
Polling bit:1 (request a status report)
Length indicator 0 (octets):9
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (9 octets):

[0]C5 91 BE 71 0D 21 00 00
[8]00
Padding associated with length indicator 1 (5 octets):

[0]55 55 55 55 55

#### MAC_DATA_REQ

RLC MAC @ 00:00:49.170

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 62

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:3

#### PHY_DATA_REQ

MAC PHY @ 00:00:49.170

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 62

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]10 20 03 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### MAC_DATA_REQ

RLC MAC @ 00:00:49.230

Category: Configuration
BTS unit: 1:
Channel No: 3 Name: DCCH
CFN: 68

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 2D 0B FE 82 24 46 68
[8]80 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:5
Polling bit:1 (request a status report)
Length indicator 0 (octets):5
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (5 octets):

[0]82 24 46 68 80
Padding associated with length indicator 1 (9 octets):

[0]00 00 00 00 00 00 00 00
[8]00

#### PHY_DATA_REQ

MAC PHY @ 00:00:49.230

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 68

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 02 D0 BF E8 22 44 66
[8]88 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 2D 0B FE 82 24 46 68
[8]80 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:00:49.290

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 54

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 06 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 60 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### MAC_DATA_IND

MAC RLC @ 00:00:49.290

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 54

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 60 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:6

#### PHY_DATA_IND

PHY MAC @ 00:00:49.300

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 55

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 02 D1 5F ED 6F 6F 71
[8]E0 EC 80 08 40 18 05 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 2D 15 FE D6 F6 F7 1E
[8]0E C8 00 84 01 80 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:00:49.300

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 55

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 2D 15 FE D6 F6 F7 1E
[8]0E C8 00 84 01 80 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:5
Polling bit:1 (request a status report)
Length indicator 0 (octets):10
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (10 octets):

[0]D6 F6 F7 1E 0E C8 00 84
[8]01 80
Padding associated with length indicator 1 (4 octets):

[0]55 55 55 55

#### RLC_AM_DATA_IND: uplinkDirectTransfer

RLC RRC @ 00:00:49.310

Channel No: 3 Name: DCCH

Message Details:

UL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode: 10101101111011011110111000111100

rrc_MessageSequenceNumber: 1

message:

uplinkDirectTransfer:

cn_DomainIdentity: ps_domain_CN_DomainIdentity [enum=1]

nas_Message: 0803

measuredResultsOnRACH: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]D6 F6 F7 1E 0E C8 00 84
[8]01 80

#### RRC_DATA_IND: gmm:attachComplete

RRC NAS @ 00:00:49.310

Cell ID: -1

Message Details:

ATTACHCOMPLETE:

skipIndicator: 0000

gMMProtocolDiscriminator: 1000

msgType: 00000011

#### MAC_DATA_REQ

RLC MAC @ 00:00:49.310

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 76

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 60 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:6

#### PHY_DATA_REQ

MAC PHY @ 00:00:49.310

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 76

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 06 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 60 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### CMAC Integrity Check Request

RRC MAC @ 00:00:49.330

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000001
Data:

[0]00 00 00 01
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:0 (UE to RNC)
Message Length (bits):80
Message:

[0]80 00 00 01 86 C8 00 84
[8]01 80

#### CMAC Integrity Check Result

MAC RRC @ 00:00:49.330

Message Details:

Integrity Check Result:

MAC-I:10101101111011011110111000111100
Data:

[0]AD ED EE 3C

#### PHY_DATA_IND

PHY MAC @ 00:00:49.500

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 75

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 06 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 60 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### MAC_DATA_IND

MAC RLC @ 00:00:49.500

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 75

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 60 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:6

#### PHY_DATA_IND

PHY MAC @ 00:00:49.510

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 76

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 02 D1 5F ED 6F 6F 71
[8]E0 EC 80 08 40 18 05 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 2D 15 FE D6 F6 F7 1E
[8]0E C8 00 84 01 80 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:00:49.510

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 76

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 2D 15 FE D6 F6 F7 1E
[8]0E C8 00 84 01 80 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:5
Polling bit:1 (request a status report)
Length indicator 0 (octets):10
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (10 octets):

[0]D6 F6 F7 1E 0E C8 00 84
[8]01 80
Padding associated with length indicator 1 (4 octets):

[0]55 55 55 55

#### MAC_DATA_REQ

RLC MAC @ 00:00:49.520

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 97

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 60 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:6

#### PHY_DATA_REQ

MAC PHY @ 00:00:49.520

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 97

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 06 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 60 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### CMAC Integrity Check Request

RRC MAC @ 00:00:50.350

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000001
Data:

[0]00 00 00 01
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:1 (RNC to UE)
Message Length (bits):56
Message:

[0]80 00 00 00 83 C8 00

#### CMAC Integrity Check Result

MAC RRC @ 00:00:50.350

Message Details:

Integrity Check Result:

MAC-I:11101100100111000001011111010011
Data:

[0]EC 9C 17 D3

#### RLC_UM_DATA_REQ

RRC LLA @ 00:00:50.350

Channel ID: Rb1
Cell ID: -1

Message Details:

RLC_UM_DATA_REQ:

cellId:-1

routingInfo:

rB_Identity:1

uM_message:

dL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode:00000000000000000000000000000000
rrc_MessageSequenceNumber:0

message: (DL_DCCH_MessageType)

rrcConnectionRelease:

r3:

rrcConnectionRelease_r3: (RRCConnectionRelease_r3_IEs)

rrc_TransactionIdentifier:0
n_308:1
releaseCause:normalEvent

rplmn_information: Omit

laterNonCriticalExtensions: Omit

specialLI:false

#### RLC_UM_DATA_REQ: rrcConnectionRelease

LLA RLC @ 00:00:50.350

Channel No: 1 Name: DCCH

Message Details:

DL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode: 11101100100111000001011111010011

rrc_MessageSequenceNumber: 1

message:

rrcConnectionRelease:

r3:

rrcConnectionRelease_r3:

rrc_TransactionIdentifier: 0

n_308: 1

releaseCause: normalEvent_ReleaseCause [enum=0]

rplmn_information: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]F6 4E 0B E9 8B C8 00

#### MAC_DATA_REQ

RLC MAC @ 00:00:50.470

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 192

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]01 0F FE F6 4E 0B E9 8B
[8]C8 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

Sequence number:0
Length indicator 0 (octets):7
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (7 octets):

[0]F6 4E 0B E9 8B C8 00
Padding associated with length indicator 1 (8 octets):

[0]00 00 00 00 00 00 00 00

#### PHY_DATA_REQ

MAC PHY @ 00:00:50.470

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 192

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]00 10 FF EF 64 E0 BE 98
[8]BC 80 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:0
MAC SDU (144 bits):

[0]01 0F FE F6 4E 0B E9 8B
[8]C8 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:00:50.710

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 196

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]00 10 DF EF BF 16 16 70
[8]C4 05 55 55 55 55 55 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:0
MAC SDU (144 bits):

[0]01 0D FE FB F1 61 67 0C
[8]40 55 55 55 55 55 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:00:50.710

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 196

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]01 0D FE FB F1 61 67 0C
[8]40 55 55 55 55 55 55 55
[16]55 55

RLC PDU (decoded):

Sequence number:0
Length indicator 0 (octets):6
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (6 octets):

[0]FB F1 61 67 0C 40
Padding associated with length indicator 1 (9 octets):

[0]55 55 55 55 55 55 55 55
[8]55

#### CMAC Integrity Check Request

RRC MAC @ 00:00:50.740

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000001
Data:

[0]00 00 00 01
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:0 (UE to RNC)
Message Length (bits):48
Message:

[0]80 00 00 00 84 40

#### RLC_UM_DATA_IND: rrcConnectionReleaseComplete

RLC LLA @ 00:00:50.740

Channel No: 1 Name: DCCH

Message Details:

UL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode: 11110111111000101100001011001110

rrc_MessageSequenceNumber: 1

message:

rrcConnectionReleaseComplete:

rrc_TransactionIdentifier: 0

errorIndication: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]FB F1 61 67 0C 40

#### CMAC Integrity Check Result

MAC RRC @ 00:00:50.740

Message Details:

Integrity Check Result:

MAC-I:11110111111000101100001011001110
Data:

[0]F7 E2 C2 CE

#### RLC_UM_DATA_IND

LLA RRC @ 00:00:50.740

Channel ID: Rb1
Cell ID: -1

Message Details:

RLC_UM_DATA_IND:

cellId:-1

routingInfo:

rB_Identity:1

integrityResult:

integrityUsed (IntegrityStatus):i_pass

uM_message:

uL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode:11110111111000101100001011001110
rrc_MessageSequenceNumber:1

message: (UL_DCCH_MessageType)

rrcConnectionReleaseComplete:

rrc_TransactionIdentifier:0

errorIndication: (FailureCauseWithProtErr) Omit

laterNonCriticalExtensions: Omit

#### PHY_DATA_IND

PHY MAC @ 00:00:50.860

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 211

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]00 30 DF ED CD 18 3E 01
[8]44 05 55 55 55 55 55 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:0
MAC SDU (144 bits):

[0]03 0D FE DC D1 83 E0 14
[8]40 55 55 55 55 55 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:00:50.860

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 211

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]03 0D FE DC D1 83 E0 14
[8]40 55 55 55 55 55 55 55
[16]55 55

RLC PDU (decoded):

Sequence number:1
Length indicator 0 (octets):6
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (6 octets):

[0]DC D1 83 E0 14 40
Padding associated with length indicator 1 (9 octets):

[0]55 55 55 55 55 55 55 55
[8]55

#### CMAC Integrity Check Request

RRC MAC @ 00:00:50.880

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000010
Data:

[0]00 00 00 02
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:0 (UE to RNC)
Message Length (bits):48
Message:

[0]80 00 00 00 84 40

#### RLC_UM_DATA_IND: rrcConnectionReleaseComplete

RLC LLA @ 00:00:50.880

Channel No: 1 Name: DCCH

Message Details:

UL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode: 10111001101000110000011111000000

rrc_MessageSequenceNumber: 2

message:

rrcConnectionReleaseComplete:

rrc_TransactionIdentifier: 0

errorIndication: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]DC D1 83 E0 14 40

#### CMAC Integrity Check Result

MAC RRC @ 00:00:50.880

Message Details:

Integrity Check Result:

MAC-I:10111001101000110000011111000000
Data:

[0]B9 A3 07 C0

#### RLC_UM_DATA_IND

LLA RRC @ 00:00:50.880

Channel ID: Rb1
Cell ID: -1

Message Details:

RLC_UM_DATA_IND:

cellId:-1

routingInfo:

rB_Identity:1

integrityResult:

integrityUsed (IntegrityStatus):i_pass

uM_message:

uL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode:10111001101000110000011111000000
rrc_MessageSequenceNumber:2

message: (UL_DCCH_MessageType)

rrcConnectionReleaseComplete:

rrc_TransactionIdentifier:0

errorIndication: (FailureCauseWithProtErr) Omit

laterNonCriticalExtensions: Omit

#### CRLC_Config_REQ

RRC LLA @ 00:00:50.880

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:1

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC UM Channel Release REQ

LLA RLC @ 00:00:50.920

BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 237

Message Details:

#### CRLC UM Channel Release CNF

RLC LLA @ 00:00:50.920

BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 237

Message Details:

#### CPHY_OUTSYNC_IND

PHY RRC @ 00:00:50.930

BTS unit: 1:1
Channel No: 0 Name: U_DPCH
CFN: 238

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:00:50.930

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:1

#### CRLC_Config_REQ

RRC LLA @ 00:00:50.930

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:2

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC AM Channel Release REQ

LLA RLC @ 00:00:50.950

BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 240

Message Details:

#### CRLC AM Channel Release CNF

RLC LLA @ 00:00:50.950

BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 240

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:00:50.970

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:2

#### CRLC_Config_REQ

RRC LLA @ 00:00:50.970

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:3

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC AM Channel Release REQ

LLA RLC @ 00:00:51.110

BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 0

Message Details:

#### CRLC AM Channel Release CNF

RLC LLA @ 00:00:51.110

BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 0

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:00:51.150

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:3

#### CRLC_Config_REQ

RRC LLA @ 00:00:51.150

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:4

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC AM Channel Release REQ

LLA RLC @ 00:00:51.270

BTS unit: 1:1
Channel No: 4 Name: DCCH
CFN: 16

Message Details:

#### CRLC AM Channel Release CNF

RLC LLA @ 00:00:51.270

BTS unit: 1:1
Channel No: 4 Name: DCCH
CFN: 16

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:00:51.290

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:4

#### CRLC_Config_REQ

RRC LLA @ 00:00:51.290

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:1

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode)

dl_UM_RLC_Mode:

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):136

dl_RLCModeInfo: (UL_RLC_Mode)

ul_UM_RLC_Mode:

transmissionRLC_Discard:

timerBasedNoExplicit (NoExplicitDiscard):dt100

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity):1
dLlogicalChannelIdentity (LogicalChannelIdentity):1
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC UM Channel Establish REQ

LLA RLC @ 00:00:51.360

BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 25

Message Details:

Configuration Parameters:

PU Size In Bits:136

#### CRLC UM Channel Establish CNF

RLC LLA @ 00:00:51.360

BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 25

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:00:51.400

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:1

#### CRLC_Config_REQ

RRC LLA @ 00:00:51.400

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:2

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode)

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):128

dl_RLCModeInfo: (UL_RLC_Mode)

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity):2
dLlogicalChannelIdentity (LogicalChannelIdentity):2
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC AM Channel Establish REQ

LLA RLC @ 00:00:51.430

BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 32

Message Details:

Configuration Parameters:

PU Size In Bits:128

Timer Parameters:

Poll (ms):200
Poll Prohibit (ms):0
EPC (ms):0
Discard (ms):0
Poll Periodic (ms):0
Status Prohibit (ms):0
Status Periodic (ms):0
Reset (ms):500
MRW (ms):0

Protocol Parameters:

Max Dat:15
Poll PU:0
Poll SDU:1
Poll Window:99
Max Reset:1
Tx Window Size:32
Rx Window Size:32
Max MRW:0
SDU Discard Mode:No discard

Polling Triggers:

Last PU In Buffer:On
Last PU In Retransmission Buffer:On
Poll Timer:On
Every Poll-PU PU:Off
Every Poll-SDU SDU:On
Poll-Window Percent Of Transmission Buffer:On
Timer Based:Off

Status Triggers:

Missing PU:On
Timer Based:Off
EPC Mechanism:Off

#### CRLC AM Channel Establish CNF

RLC LLA @ 00:00:51.430

BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 32

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:00:51.440

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:2

#### CRLC_Config_REQ

RRC LLA @ 00:00:51.440

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:3

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode)

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):128

dl_RLCModeInfo: (UL_RLC_Mode)

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity):3
dLlogicalChannelIdentity (LogicalChannelIdentity):3
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC AM Channel Establish REQ

LLA RLC @ 00:00:51.570

BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 46

Message Details:

Configuration Parameters:

PU Size In Bits:128

Timer Parameters:

Poll (ms):200
Poll Prohibit (ms):0
EPC (ms):0
Discard (ms):0
Poll Periodic (ms):0
Status Prohibit (ms):0
Status Periodic (ms):0
Reset (ms):500
MRW (ms):0

Protocol Parameters:

Max Dat:15
Poll PU:0
Poll SDU:1
Poll Window:99
Max Reset:1
Tx Window Size:32
Rx Window Size:32
Max MRW:0
SDU Discard Mode:No discard

Polling Triggers:

Last PU In Buffer:On
Last PU In Retransmission Buffer:On
Poll Timer:On
Every Poll-PU PU:Off
Every Poll-SDU SDU:On
Poll-Window Percent Of Transmission Buffer:On
Timer Based:Off

Status Triggers:

Missing PU:On
Timer Based:Off
EPC Mechanism:Off

#### CRLC AM Channel Establish CNF

RLC LLA @ 00:00:51.570

BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 46

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:00:51.580

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:3

#### CRLC_Config_REQ

RRC LLA @ 00:00:51.580

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:4

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode)

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):128

dl_RLCModeInfo: (UL_RLC_Mode)

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity):4
dLlogicalChannelIdentity (LogicalChannelIdentity):4
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC AM Channel Establish REQ

LLA RLC @ 00:00:51.750

BTS unit: 1:1
Channel No: 4 Name: DCCH
CFN: 64

Message Details:

Configuration Parameters:

PU Size In Bits:128

Timer Parameters:

Poll (ms):200
Poll Prohibit (ms):0
EPC (ms):0
Discard (ms):0
Poll Periodic (ms):0
Status Prohibit (ms):0
Status Periodic (ms):0
Reset (ms):500
MRW (ms):0

Protocol Parameters:

Max Dat:15
Poll PU:0
Poll SDU:1
Poll Window:99
Max Reset:1
Tx Window Size:32
Rx Window Size:32
Max MRW:0
SDU Discard Mode:No discard

Polling Triggers:

Last PU In Buffer:On
Last PU In Retransmission Buffer:On
Poll Timer:On
Every Poll-PU PU:Off
Every Poll-SDU SDU:On
Poll-Window Percent Of Transmission Buffer:On
Timer Based:Off

Status Triggers:

Missing PU:On
Timer Based:Off
EPC Mechanism:Off

#### CRLC AM Channel Establish CNF

RLC LLA @ 00:00:51.750

BTS unit: 1:1
Channel No: 4 Name: DCCH
CFN: 64

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:00:51.790

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:4

#### AT_CmdReq

RRC LLA @ 00:00:51.790

Message Details:

AT_CmdReq:

cmd (IA5String):AT+CGEQREQ=1,2,64,64,,,1,320,"1E4","1E5",1,,3<CR>
sMS_BlockMode (HEXSTRING):

Omit

#### AT_CmdCnf

LLA RRC @ 00:00:55.160

Message Details:

AT_CmdCnf:

result: Omit
resultString (IA5String):<CR><LF>OK<CR><LF>
sMS_BlockMode (HEXSTRING):

Omit

#### AT_CmdReq

RRC LLA @ 00:00:55.160

Message Details:

AT_CmdReq:

cmd (IA5String):AT+CGDCONT=1,"IP","ABCDEF","200.1.1.80",0,0<CR>
sMS_BlockMode (HEXSTRING):

Omit

#### AT_CmdCnf

LLA RRC @ 00:00:56.440

Message Details:

AT_CmdCnf:

result: Omit
resultString (IA5String):<CR><LF>OK<CR><LF>
sMS_BlockMode (HEXSTRING):

Omit

#### AT_CmdReq

RRC LLA @ 00:00:56.440

Message Details:

AT_CmdReq:

cmd (IA5String):AT+CGACT=1,1<CR>
sMS_BlockMode (HEXSTRING):

Omit

#### AT_CmdCnf

LLA RRC @ 00:00:57.160

Message Details:

AT_CmdCnf:

result: Omit
resultString (IA5String):<CR><LF>OK<CR><LF>
sMS_BlockMode (HEXSTRING):

Omit

#### PHY_DATA_IND

PHY MAC @ 00:01:00.750

BTS unit: 1:1
Channel No: 0 Name: U_RACH
CFN: 176

Message Details:

TFI:0
TB set size:168
TB size:168
TB set (raw):

[0]08 44 48 8C D1 00 04 02
[8]00 02 20 00 00 00 00 00
[16]00 00 00 00 00 00

TB set (decoded):

TB 0:

TCTF:0
MAC SDU (166 bits):

[0]21 11 22 33 44 00 10 08
[8]00 08 80 00 00 00 00 00
[16]00 00 00 00 00

#### MAC_DATA_IND

MAC RLC @ 00:01:00.750

Category: Configuration
BTS unit: 1:1
Channel No: 0 Name: CCCH
CFN: 176

Message Details:

RLC PDU size (bits):166
RLC PDU (raw):

[0]21 11 22 33 44 00 10 08
[8]00 08 80 00 00 00 00 00
[16]00 00 00 00 00

#### RLC_TR_DATA_IND: rrcConnectionRequest

RLC LLA @ 00:01:00.790

Channel No: 0 Name: CCCH

Message Details:

UL_CCCH_Message:

integrityCheckInfo: Omitted

message:

rrcConnectionRequest:

initialUE_Identity:

tmsi_and_LAI:

tmsi: 00010001001000100011001101000100

lai:

plmn_Identity:

mcc:

MCC.element: 0

MCC.element: 0

MCC.element: 1

mnc:

MNC.element: 0

MNC.element: 1

lac: 0000000000000001

establishmentCause: originatingInteractiveCall_EstablishmentCause [enum=2]

protocolErrorIndicator: noError_ProtocolErrorIndicator [enum=0]

measuredResultsOnRACH: Omitted

v3d0NonCriticalExtensions: Omitted

Layer 3 SDU:

[0]21 11 22 33 44 00 10 08
[8]00 08 80 00 00 00 00 00
[16]00 00 00 00 00

#### RLC_TR_DATA_IND

LLA RRC @ 00:01:00.790

Channel ID: Rb0
Cell ID: 0

Message Details:

RLC_TR_DATA_IND:

cellId:0

routingInfo:

rB_Identity:0

tM_message:

uL_CCCH_Message:

integrityCheckInfo: Omit

message: (UL_CCCH_MessageType)

rrcConnectionRequest:

initialUE_Identity:

tmsi_and_LAI: (TMSI_and_LAI_GSM_MAP)

tmsi (TMSI_GSM_MAP):00010001001000100011001101000100

lai:

plmn_Identity:

mcc:

Digit:0
Digit:0
Digit:1

mnc:

Digit:0
Digit:1

lac:0000000000000001

establishmentCause:originatingInteractiveCall
protocolErrorIndicator:noError

measuredResultsOnRACH: Omit

v3d0NonCriticalExtensions: Omit

#### RLC_UM_DATA_REQ

RRC LLA @ 00:01:00.790

Channel ID: Rb0
Cell ID: 0

Message Details:

RLC_UM_DATA_REQ:

cellId:0

routingInfo:

rB_Identity:0

uM_message:

dL_CCCH_Message:

integrityCheckInfo: Omit

message: (DL_CCCH_MessageType)

rrcConnectionSetup:

r3:

rrcConnectionSetup_r3: (RRCConnectionSetup_r3_IEs)

initialUE_Identity:

tmsi_and_LAI: (TMSI_and_LAI_GSM_MAP)

tmsi (TMSI_GSM_MAP):00010001001000100011001101000100

lai:

plmn_Identity:

mcc:

Digit:0
Digit:0
Digit:1

mnc:

Digit:0
Digit:1

lac:0000000000000001

rrc_TransactionIdentifier:0
activationTime: Omit

new_U_RNTI: (U_RNTI)

srnc_Identity:000000000001
s_RNTI:00000000000000000001

new_c_RNTI (C_RNTI): Omit
rrc_StateIndicator:cell_DCH
utran_DRX_CycleLengthCoeff (UTRAN_DRX_CycleLengthCoefficient):9

capabilityUpdateRequirement:

ue_RadioCapabilityFDDUpdateRequirement:true
ue_RadioCapabilityTDDUpdateRequirement:false

systemSpecificCapUpdateReqList:

SystemSpecificCapUpdateReq:gsm

srb_InformationSetupList: (SRB_InformationSetupList2)

SRB_InformationSetup:

rb_Identity: Omit

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_UM_RLC_Mode:

transmissionRLC_Discard: Omit

dl_RLC_Mode:

dl_UM_RLC_Mode:

rb_MappingInfo:

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

dch (TransportChannelIdentity):5

logicalChannelIdentity:1

rlc_SizeList:

configured:

mac_LogicalChannelPriority:1

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

dch (TransportChannelIdentity):10

logicalChannelIdentity:1

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

rach:

logicalChannelIdentity:1

rlc_SizeList:

explicitList: (RLC_SizeExplicitList)

RLC_SizeInfo:

rlc_SizeIndex:1

mac_LogicalChannelPriority:1

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

fach:

logicalChannelIdentity:1

SRB_InformationSetup:

rb_Identity: Omit

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

rb_MappingInfo:

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

dch (TransportChannelIdentity):5

logicalChannelIdentity:2

rlc_SizeList:

configured:

mac_LogicalChannelPriority:2

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

dch (TransportChannelIdentity):10

logicalChannelIdentity:2

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

rach:

logicalChannelIdentity:2

rlc_SizeList:

explicitList: (RLC_SizeExplicitList)

RLC_SizeInfo:

rlc_SizeIndex:1

mac_LogicalChannelPriority:2

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

fach:

logicalChannelIdentity:2

SRB_InformationSetup:

rb_Identity: Omit

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

rb_MappingInfo:

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

dch (TransportChannelIdentity):5

logicalChannelIdentity:3

rlc_SizeList:

configured:

mac_LogicalChannelPriority:3

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

dch (TransportChannelIdentity):10

logicalChannelIdentity:3

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

rach:

logicalChannelIdentity:3

rlc_SizeList:

explicitList: (RLC_SizeExplicitList)

RLC_SizeInfo:

rlc_SizeIndex:1

mac_LogicalChannelPriority:3

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

fach:

logicalChannelIdentity:3

SRB_InformationSetup:

rb_Identity: Omit

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

rb_MappingInfo:

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

dch (TransportChannelIdentity):5

logicalChannelIdentity:4

rlc_SizeList:

configured:

mac_LogicalChannelPriority:4

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

dch (TransportChannelIdentity):10

logicalChannelIdentity:4

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

rach:

logicalChannelIdentity:4

rlc_SizeList:

explicitList: (RLC_SizeExplicitList)

RLC_SizeInfo:

rlc_SizeIndex:1

mac_LogicalChannelPriority:4

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

fach:

logicalChannelIdentity:4

ul_CommonTransChInfo:

tfc_Subset: Omit

prach_TFCS: (TFCS) Omit

modeSpecificInfo:

fdd:

ul_TFCS: (TFCS)

normalTFCI_Signalling: (ExplicitTFCS_Configuration)

complete: (TFCS_ReconfAdd)

ctfcSize:

ctfc2Bit:

:

ctfc2:0

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc2:1

powerOffsetInformation:

gainFactorInformation:

signalledGainFactors:

modeSpecificInfo:

fdd:

gainFactorBetaC (GainFactor):11

gainFactorBetaD (GainFactor):15
referenceTFC_ID:0

powerOffsetPp_m: Omit

ul_AddReconfTransChInfoList:

UL_AddReconfTransChInformation:

ul_TransportChannelType (UL_TrCH_Type):dch
transportChannelIdentity:5

transportFormatSet:

dedicatedTransChTFS:

tti:

tti10: (DedicatedDynamicTF_InfoList)

DedicatedDynamicTF_Info:

rlc_Size:

bitMode: (BitModeRLC_SizeInfo)

sizeType2:

part1:2
part2: Omit

numberOfTbSizeList:

NumberOfTransportBlocks:

zero:

NumberOfTransportBlocks:

one:

logicalChannelList:

allSizes:

semistaticTF_Information:

channelCodingType:

convolutional (CodingRate):third

rateMatchingAttribute:192
crc_Size:crc16

dl_CommonTransChInfo:

sccpch_TFCS: (TFCS) Omit

modeSpecificInfo:

fdd:

dl_Parameters:

sameAsUL:

dl_AddReconfTransChInfoList:

DL_AddReconfTransChInformation:

dl_TransportChannelType (DL_TrCH_Type):dch
dl_transportChannelIdentity (TransportChannelIdentity):10

tfs_SignallingMode:

sameAsULTrCH: (UL_TransportChannelIdentity)

ul_TransportChannelType (UL_TrCH_Type):dch
ul_TransportChannelIdentity (TransportChannelIdentity):5

dch_QualityTarget: (QualityTarget)

bler_QualityValue:-20

dummy: (TM_SignallingInfo) Omit

frequencyInfo: Omit

maxAllowedUL_TX_Power: Omit

ul_ChannelRequirement:

ul_DPCH_Info:

ul_DPCH_PowerControlInfo:

fdd:

dpcch_PowerOffset:-40
pc_Preamble:1
sRB_delay:7

powerControlAlgorithm:

algorithm1 (TPC_StepSizeFDD):1

modeSpecificInfo:

fdd:

scramblingCodeType:longSC
scramblingCode (UL_ScramblingCode):0
numberOfDPDCH: Omit
spreadingFactor:sf64
tfci_Existence:true
numberOfFBI_Bits: Omit
puncturingLimit:pl1

dl_CommonInformation:

dl_DPCH_InfoCommon:

cfnHandling:

initialise:

cfntargetsfnframeoffset: Omit

modeSpecificInfo:

fdd:

dl_DPCH_PowerControlInfo:

modeSpecificInfo:

fdd:

dpc_Mode:singleTPC

powerOffsetPilot_pdpdch:0

dl_rate_matching_restriction: Omit

spreadingFactorAndPilot: (SF512_AndPilot)

sfd128 (PilotBits128):pb4

positionFixedOrFlexible:fixed
tfci_Existence:false

modeSpecificInfo:

fdd:

defaultDPCH_OffsetValue (DefaultDPCH_OffsetValueFDD):0

dpch_CompressedModeInfo: Omit

tx_DiversityMode:noDiversity

ssdt_Information: Omit

dl_InformationPerRL_List:

DL_InformationPerRL:

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode:100

pdsch_SHO_DCH_Info: Omit

pdsch_CodeMapping: Omit

dl_DPCH_InfoPerRL:

fdd:

pCPICH_UsageForChannelEst:mayBeUsed
dpch_FrameOffset:0

secondaryCPICH_Info: Omit

dl_ChannelisationCodeList:

DL_ChannelisationCode:

secondaryScramblingCode:1

sf_AndCodeNumber: (SF512_AndCodeNumber)

sf128:0

scramblingCodeChange:noCodeChange

tpc_CombinationIndex:0
ssdt_CellIdentity: Omit
closedLoopTimingAdjMode: Omit

sccpch_InfoforFACH: Omit

laterNonCriticalExtensions: Omit

specialLI:true

#### RLC_UM_DATA_REQ: rrcConnectionSetup

LLA RLC @ 00:01:00.790

Channel No: 1 Name: CCCH

Message Details:

DL_CCCH_Message:

integrityCheckInfo: Omitted

message:

rrcConnectionSetup:

r3:

rrcConnectionSetup_r3:

initialUE_Identity:

tmsi_and_LAI:

tmsi: 00010001001000100011001101000100

lai:

plmn_Identity:

mcc:

MCC.element: 0

MCC.element: 0

MCC.element: 1

mnc:

MNC.element: 0

MNC.element: 1

lac: 0000000000000001

rrc_TransactionIdentifier: 0

activationTime: Omitted

new_U_RNTI:

srnc_Identity: 000000000001

s_RNTI: 00000000000000000001

new_c_RNTI: Omitted

rrc_StateIndicator: cell_DCH_RRC_StateIndicator [enum=0]

utran_DRX_CycleLengthCoeff: 9

capabilityUpdateRequirement:

ue_RadioCapabilityFDDUpdateRequirement: 1

ue_RadioCapabilityTDDUpdateRequirement: 0

systemSpecificCapUpdateReqList:

SystemSpecificCapUpdateReqList.element: gsm_SystemSpecificCapUpdateReq [enum=0]

srb_InformationSetupList:

SRB_InformationSetupList2.element:

rb_Identity: Omitted

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_UM_RLC_Mode:

transmissionRLC_Discard: Omitted

dl_RLC_Mode:

dl_UM_RLC_Mode: NULL

rb_MappingInfo:

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

dch: 5

logicalChannelIdentity: 1

rlc_SizeList:

configured: NULL

mac_LogicalChannelPriority: 1

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

dch: 10

logicalChannelIdentity: 1

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

rach: NULL

logicalChannelIdentity: 1

rlc_SizeList:

explicitList:

RLC_SizeExplicitList.element:

rlc_SizeIndex: 1

mac_LogicalChannelPriority: 1

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

fach: NULL

logicalChannelIdentity: 1

SRB_InformationSetupList2.element:

rb_Identity: Omitted

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard: dat15_MaxDAT [enum=10]

transmissionWindowSize: tw32_TransmissionWindowSize [enum=3]

timerRST: tr500_TimerRST [enum=9]

max_RST: rst1_MaxRST [enum=0]

pollingInfo:

timerPollProhibit: tpp200_TimerPollProhibit [enum=19]

timerPoll: tp200_TimerPoll [enum=19]

poll_PDU: Omitted

poll_SDU: sdu1_Poll_SDU [enum=0]

lastTransmissionPDU_Poll: 1

lastRetransmissionPDU_Poll: 1

pollWindow: pw99_PollWindow [enum=7]

timerPollPeriodic: Omitted

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery: 1

receivingWindowSize: rw32_ReceivingWindowSize [enum=3]

dl_RLC_StatusInfo:

timerStatusProhibit: tsp200_TimerStatusProhibit [enum=19]

timerEPC: Omitted

missingPDU_Indicator: 1

timerStatusPeriodic: Omitted

rb_MappingInfo:

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

dch: 5

logicalChannelIdentity: 2

rlc_SizeList:

configured: NULL

mac_LogicalChannelPriority: 2

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

dch: 10

logicalChannelIdentity: 2

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

rach: NULL

logicalChannelIdentity: 2

rlc_SizeList:

explicitList:

RLC_SizeExplicitList.element:

rlc_SizeIndex: 1

mac_LogicalChannelPriority: 2

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

fach: NULL

logicalChannelIdentity: 2

SRB_InformationSetupList2.element:

rb_Identity: Omitted

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard: dat15_MaxDAT [enum=10]

transmissionWindowSize: tw32_TransmissionWindowSize [enum=3]

timerRST: tr500_TimerRST [enum=9]

max_RST: rst1_MaxRST [enum=0]

pollingInfo:

timerPollProhibit: tpp200_TimerPollProhibit [enum=19]

timerPoll: tp200_TimerPoll [enum=19]

poll_PDU: Omitted

poll_SDU: sdu1_Poll_SDU [enum=0]

lastTransmissionPDU_Poll: 1

lastRetransmissionPDU_Poll: 1

pollWindow: pw99_PollWindow [enum=7]

timerPollPeriodic: Omitted

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery: 1

receivingWindowSize: rw32_ReceivingWindowSize [enum=3]

dl_RLC_StatusInfo:

timerStatusProhibit: tsp200_TimerStatusProhibit [enum=19]

timerEPC: Omitted

missingPDU_Indicator: 1

timerStatusPeriodic: Omitted

rb_MappingInfo:

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

dch: 5

logicalChannelIdentity: 3

rlc_SizeList:

configured: NULL

mac_LogicalChannelPriority: 3

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

dch: 10

logicalChannelIdentity: 3

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

rach: NULL

logicalChannelIdentity: 3

rlc_SizeList:

explicitList:

RLC_SizeExplicitList.element:

rlc_SizeIndex: 1

mac_LogicalChannelPriority: 3

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

fach: NULL

logicalChannelIdentity: 3

SRB_InformationSetupList2.element:

rb_Identity: Omitted

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard: dat15_MaxDAT [enum=10]

transmissionWindowSize: tw32_TransmissionWindowSize [enum=3]

timerRST: tr500_TimerRST [enum=9]

max_RST: rst1_MaxRST [enum=0]

pollingInfo:

timerPollProhibit: tpp200_TimerPollProhibit [enum=19]

timerPoll: tp200_TimerPoll [enum=19]

poll_PDU: Omitted

poll_SDU: sdu1_Poll_SDU [enum=0]

lastTransmissionPDU_Poll: 1

lastRetransmissionPDU_Poll: 1

pollWindow: pw99_PollWindow [enum=7]

timerPollPeriodic: Omitted

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery: 1

receivingWindowSize: rw32_ReceivingWindowSize [enum=3]

dl_RLC_StatusInfo:

timerStatusProhibit: tsp200_TimerStatusProhibit [enum=19]

timerEPC: Omitted

missingPDU_Indicator: 1

timerStatusPeriodic: Omitted

rb_MappingInfo:

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

dch: 5

logicalChannelIdentity: 4

rlc_SizeList:

configured: NULL

mac_LogicalChannelPriority: 4

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

dch: 10

logicalChannelIdentity: 4

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

rach: NULL

logicalChannelIdentity: 4

rlc_SizeList:

explicitList:

RLC_SizeExplicitList.element:

rlc_SizeIndex: 1

mac_LogicalChannelPriority: 4

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

fach: NULL

logicalChannelIdentity: 4

ul_CommonTransChInfo:

tfc_Subset: Omitted

prach_TFCS: Omitted

modeSpecificInfo:

fdd:

ul_TFCS:

normalTFCI_Signalling:

complete:

ctfcSize:

ctfc2Bit:

ctfc2Bit.noName:

ctfc2: 0

powerOffsetInformation:

gainFactorInformation:

computedGainFactors: 0

powerOffsetPp_m: Omitted

ctfc2Bit.noName:

ctfc2: 1

powerOffsetInformation:

gainFactorInformation:

signalledGainFactors:

modeSpecificInfo:

fdd:

gainFactorBetaC: 11

gainFactorBetaD: 15

referenceTFC_ID: 0

powerOffsetPp_m: Omitted

ul_AddReconfTransChInfoList:

UL_AddReconfTransChInfoList.element:

ul_TransportChannelType: dch_UL_TrCH_Type [enum=0]

transportChannelIdentity: 5

transportFormatSet:

dedicatedTransChTFS:

tti:

tti10:

DedicatedDynamicTF_InfoList.element:

rlc_Size:

bitMode:

sizeType2:

part1: 2

part2: Omitted

numberOfTbSizeList:

numberOfTbSizeList.element:

zero: NULL

numberOfTbSizeList.element:

one: NULL

logicalChannelList:

allSizes: NULL

semistaticTF_Information:

channelCodingType:

convolutional: third_CodingRate [enum=1]

rateMatchingAttribute: 192

crc_Size: crc16_CRC_Size [enum=3]

dl_CommonTransChInfo:

sccpch_TFCS: Omitted

modeSpecificInfo:

fdd:

dl_Parameters:

sameAsUL: NULL

dl_AddReconfTransChInfoList:

DL_AddReconfTransChInfoList.element:

dl_TransportChannelType: dch_DL_TrCH_Type [enum=0]

dl_transportChannelIdentity: 10

tfs_SignallingMode:

sameAsULTrCH:

ul_TransportChannelType: dch_UL_TrCH_Type [enum=0]

ul_TransportChannelIdentity: 5

dch_QualityTarget:

bler_QualityValue: -20

dummy: Omitted

frequencyInfo: Omitted

maxAllowedUL_TX_Power: Omitted

ul_ChannelRequirement:

ul_DPCH_Info:

ul_DPCH_PowerControlInfo:

fdd:

dpcch_PowerOffset: -40

pc_Preamble: 1

sRB_delay: 7

powerControlAlgorithm:

algorithm1: 1

modeSpecificInfo:

fdd:

scramblingCodeType: longSC_ScramblingCodeType [enum=1]

scramblingCode: 0

numberOfDPDCH: Default

spreadingFactor: sf64_SpreadingFactor [enum=4]

tfci_Existence: 1

numberOfFBI_Bits: Omitted

puncturingLimit: pl1_PuncturingLimit [enum=15]

dl_CommonInformation:

dl_DPCH_InfoCommon:

cfnHandling:

initialise:

cfntargetsfnframeoffset: Omitted

modeSpecificInfo:

fdd:

dl_DPCH_PowerControlInfo:

modeSpecificInfo:

fdd:

dpc_Mode: singleTPC_DPC_Mode [enum=0]

powerOffsetPilot_pdpdch: 0

dl_rate_matching_restriction: Omitted

spreadingFactorAndPilot:

sfd128: pb4_PilotBits128 [enum=0]

positionFixedOrFlexible: fixed_PositionFixedOrFlexible [enum=0]

tfci_Existence: 0

modeSpecificInfo:

fdd:

defaultDPCH_OffsetValue: 0

dpch_CompressedModeInfo: Omitted

tx_DiversityMode: noDiversity_TX_DiversityMode [enum=0]

ssdt_Information: Omitted

dl_InformationPerRL_List:

DL_InformationPerRL_List.element:

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode: 100

pdsch_SHO_DCH_Info: Omitted

pdsch_CodeMapping: Omitted

dl_DPCH_InfoPerRL:

fdd:

pCPICH_UsageForChannelEst: mayBeUsed_PCPICH_UsageForChannelEst [enum=0]

dpch_FrameOffset: 0

secondaryCPICH_Info: Omitted

dl_ChannelisationCodeList:

DL_ChannelisationCodeList.element:

secondaryScramblingCode: 1

sf_AndCodeNumber:

sf128: 0

scramblingCodeChange: noCodeChange_ScramblingCodeChange [enum=1]

tpc_CombinationIndex: 0

ssdt_CellIdentity: Omitted

closedLoopTimingAdjMode: Omitted

sccpch_InfoforFACH: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]30 E7 22 24 46 68 80 02
[8]01 00 01 00 04 00 00 4D
[16]82 69 3A 10 10 89 0D 42
[24]00 02 81 9E 8E 46 C9 A6
[32]7C 9C 4E 74 20 A5 12 3A
[40]8C 00 15 13 3D 1C 8D 93
[48]4C F9 38 9C E8 42 52 24
[56]B5 28 00 4A 46 7A 39 1B
[64]26 99 F2 71 39 D0 86 B4
[72]49 EA 70 00 D4 C8 00 06
[80]25 2B F0 02 00 08 82 23
[88]BF 66 08 98 95 A5 47 A2
[96]00 00 01 3F 90 0A 14 00
[104]02 06 40 00 0C 28 08

#### MAC_DATA_REQ

RLC MAC @ 00:01:00.870

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: CCCH
CFN: 208

Message Details:

RLC PDU size (bits):160
RLC PDU (raw):

[0]19 F8 30 E7 22 24 46 68
[8]80 02 01 00 01 00 04 00
[16]00 4D 82 69

RLC PDU (decoded):

Sequence number:12
Length indicator 0 (octets):124 (the first data octet in this RLC PDU is the first octet of a RLC SDU)
Segment associated with length indicator 0 (0 octets):

Last segment, not associated with any length indicators (18 octets):

[0]30 E7 22 24 46 68 80 02
[8]01 00 01 00 04 00 00 4D
[16]82 69

#### MAC_DATA_REQ

RLC MAC @ 00:01:00.870

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: CCCH
CFN: 208

Message Details:

RLC PDU size (bits):160
RLC PDU (raw):

[0]1A 3A 10 10 89 0D 42 00
[8]02 81 9E 8E 46 C9 A6 7C
[16]9C 4E 74 20

RLC PDU (decoded):

Sequence number:13
Last segment, not associated with any length indicators (19 octets):

[0]3A 10 10 89 0D 42 00 02
[8]81 9E 8E 46 C9 A6 7C 9C
[16]4E 74 20

#### MAC_DATA_REQ

RLC MAC @ 00:01:00.870

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: CCCH
CFN: 208

Message Details:

RLC PDU size (bits):160
RLC PDU (raw):

[0]1C A5 12 3A 8C 00 15 13
[8]3D 1C 8D 93 4C F9 38 9C
[16]E8 42 52 24

RLC PDU (decoded):

Sequence number:14
Last segment, not associated with any length indicators (19 octets):

[0]A5 12 3A 8C 00 15 13 3D
[8]1C 8D 93 4C F9 38 9C E8
[16]42 52 24

#### MAC_DATA_REQ

RLC MAC @ 00:01:00.870

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: CCCH
CFN: 208

Message Details:

RLC PDU size (bits):160
RLC PDU (raw):

[0]1E B5 28 00 4A 46 7A 39
[8]1B 26 99 F2 71 39 D0 86
[16]B4 49 EA 70

RLC PDU (decoded):

Sequence number:15
Last segment, not associated with any length indicators (19 octets):

[0]B5 28 00 4A 46 7A 39 1B
[8]26 99 F2 71 39 D0 86 B4
[16]49 EA 70

#### MAC_DATA_REQ

RLC MAC @ 00:01:00.870

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: CCCH
CFN: 208

Message Details:

RLC PDU size (bits):160
RLC PDU (raw):

[0]20 00 D4 C8 00 06 25 2B
[8]F0 02 00 08 82 23 BF 66
[16]08 98 95 A5

RLC PDU (decoded):

Sequence number:16
Last segment, not associated with any length indicators (19 octets):

[0]00 D4 C8 00 06 25 2B F0
[8]02 00 08 82 23 BF 66 08
[16]98 95 A5

#### MAC_DATA_REQ

RLC MAC @ 00:01:00.870

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: CCCH
CFN: 208

Message Details:

RLC PDU size (bits):160
RLC PDU (raw):

[0]23 23 FE 47 A2 00 00 01
[8]3F 90 0A 14 00 02 06 40
[16]00 0C 28 08

RLC PDU (decoded):

Sequence number:17
Length indicator 0 (octets):17
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (17 octets):

[0]47 A2 00 00 01 3F 90 0A
[8]14 00 02 06 40 00 0C 28
[16]08
Padding associated with length indicator 1 (0 octets):

#### PHY_DATA_REQ

MAC PHY @ 00:01:00.870

BTS unit: 1:1
Channel No: 0 Name: FACH
CFN: 208

Message Details:

TFI:2
TB set size:336
TB size:168
TB set (raw, each TB word aligned):

[0]40 19 F8 30 E7 22 24 46
[8]68 80 02 01 00 01 00 04
[16]00 00 4D 82 69 00 40 1A
[24]3A 10 10 89 0D 42 00 02
[32]81 9E 8E 46 C9 A6 7C 9C
[40]4E 74 20 00

TB set (decoded):

TB 0:

TCTF:64
MAC SDU (160 bits):

[0]19 F8 30 E7 22 24 46 68
[8]80 02 01 00 01 00 04 00
[16]00 4D 82 69

TB 1:

TCTF:64
MAC SDU (160 bits):

[0]1A 3A 10 10 89 0D 42 00
[8]02 81 9E 8E 46 C9 A6 7C
[16]9C 4E 74 20

#### PHY_DATA_REQ

MAC PHY @ 00:01:00.880

BTS unit: 1:1
Channel No: 0 Name: FACH
CFN: 209

Message Details:

TFI:2
TB set size:336
TB size:168
TB set (raw, each TB word aligned):

[0]40 1C A5 12 3A 8C 00 15
[8]13 3D 1C 8D 93 4C F9 38
[16]9C E8 42 52 24 00 40 1E
[24]B5 28 00 4A 46 7A 39 1B
[32]26 99 F2 71 39 D0 86 B4
[40]49 EA 70 00

TB set (decoded):

TB 0:

TCTF:64
MAC SDU (160 bits):

[0]1C A5 12 3A 8C 00 15 13
[8]3D 1C 8D 93 4C F9 38 9C
[16]E8 42 52 24

TB 1:

TCTF:64
MAC SDU (160 bits):

[0]1E B5 28 00 4A 46 7A 39
[8]1B 26 99 F2 71 39 D0 86
[16]B4 49 EA 70

#### PHY_DATA_REQ

MAC PHY @ 00:01:00.890

BTS unit: 1:1
Channel No: 0 Name: FACH
CFN: 210

Message Details:

TFI:2
TB set size:336
TB size:168
TB set (raw, each TB word aligned):

[0]40 20 00 D4 C8 00 06 25
[8]2B F0 02 00 08 82 23 BF
[16]66 08 98 95 A5 00 40 23
[24]23 FE 47 A2 00 00 01 3F
[32]90 0A 14 00 02 06 40 00
[40]0C 28 08 00

TB set (decoded):

TB 0:

TCTF:64
MAC SDU (160 bits):

[0]20 00 D4 C8 00 06 25 2B
[8]F0 02 00 08 82 23 BF 66
[16]08 98 95 A5

TB 1:

TCTF:64
MAC SDU (160 bits):

[0]23 23 FE 47 A2 00 00 01
[8]3F 90 0A 14 00 02 06 40
[16]00 0C 28 08

#### CPHY_SYNC_IND

PHY RRC @ 00:01:01.170

BTS unit: 1:1
Channel No: 0 Name: U_DPCH
CFN: 238

Message Details:

#### PHY_DATA_IND

PHY MAC @ 00:01:01.330

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 234

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 00 04 A0 C0 00 08 00
[8]00 5E 23 41 A2 09 09 8C
[16]D0 8C 50 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 00 4A 0C 00 00 80 00
[8]05 E2 34 1A 20 90 98 CD
[16]08 C5

#### MAC_DATA_IND

MAC RLC @ 00:01:01.330

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 234

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 00 4A 0C 00 00 80 00
[8]05 E2 34 1A 20 90 98 CD
[16]08 C5

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:0
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]4A 0C 00 00 80 00 05 E2
[8]34 1A 20 90 98 CD 08 C5

#### PHY_DATA_IND

PHY MAC @ 00:01:01.340

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 235

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 00 D1 5F E9 26 04 10
[8]00 10 00 23 1F 1F 05 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 0D 15 FE 92 60 41 00
[8]01 00 02 31 F1 F0 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:01:01.340

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 235

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 0D 15 FE 92 60 41 00
[8]01 00 02 31 F1 F0 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:1
Polling bit:1 (request a status report)
Length indicator 0 (octets):10
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (10 octets):

[0]92 60 41 00 01 00 02 31
[8]F1 F0
Padding associated with length indicator 1 (4 octets):

[0]55 55 55 55

#### MAC_DATA_REQ

RLC MAC @ 00:01:01.350

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 0

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 20 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:2

#### PHY_DATA_REQ

MAC PHY @ 00:01:01.350

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 0

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]10 20 02 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]02 00 20 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:01:01.350

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 236

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 00 01 58 0D 10 06 04
[8]06 00 02 FA 09 1A 2B 3C
[16]19 01 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 00 15 80 D1 00 60 40
[8]60 00 2F A0 91 A2 B3 C1
[16]90 10

#### MAC_DATA_IND

MAC RLC @ 00:01:01.350

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 236

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 00 15 80 D1 00 60 40
[8]60 00 2F A0 91 A2 B3 C1
[16]90 10

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:0
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]15 80 D1 00 60 40 60 00
[8]2F A0 91 A2 B3 C1 90 10

#### PHY_DATA_IND

PHY MAC @ 00:01:01.360

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 237

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 00 D0 BF E0 00 20 00
[8]04 05 55 55 55 55 55 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 0D 0B FE 00 02 00 00
[8]40 55 55 55 55 55 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:01:01.360

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 237

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 0D 0B FE 00 02 00 00
[8]40 55 55 55 55 55 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:1
Polling bit:1 (request a status report)
Length indicator 0 (octets):5
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (5 octets):

[0]00 02 00 00 40
Padding associated with length indicator 1 (9 octets):

[0]55 55 55 55 55 55 55 55
[8]55

#### RLC_AM_DATA_IND: rrcConnectionSetupComplete

RLC LLA @ 00:01:01.360

Channel No: 2 Name: DCCH

Message Details:

UL_DCCH_Message:

integrityCheckInfo: Omitted

message:

rrcConnectionSetupComplete:

rrc_TransactionIdentifier: 0

startList:

STARTList.element:

cn_DomainIdentity: ps_domain_CN_DomainIdentity [enum=1]

start_Value: 00000000000000000010

STARTList.element:

cn_DomainIdentity: cs_domain_CN_DomainIdentity [enum=0]

start_Value: 00000000000000000010

ue_RadioAccessCapability:

accessStratumReleaseIndicator: r99_AccessStratumReleaseIndicator [enum=0]

pdcp_Capability:

losslessSRNS_RelocationSupport: 1

supportForRfc2507:

supported: by8192_MaxHcContextSpace [enum=4]

rlc_Capability:

totalRLC_AM_BufferSize: kb50_TotalRLC_AM_BufferSize [enum=2]

maximumRLC_WindowSize: mws2047_MaximumRLC_WindowSize [enum=0]

maximumAM_EntityNumber: am6_MaximumAM_EntityNumberRLC_Cap [enum=3]

transportChannelCapability:

dl_TransChCapability:

maxNoBitsReceived: b5120_MaxNoBits [enum=4]

maxConvCodeBitsReceived: b1280_MaxNoBits [enum=1]

turboDecodingSupport:

supported: b5120_MaxNoBits [enum=4]

maxSimultaneousTransChs: e8_MaxSimultaneousTransChsDL [enum=1]

maxSimultaneousCCTrCH_Count: 1

maxReceivedTransportBlocks: tb16_MaxTransportBlocksDL [enum=2]

maxNumberOfTFC: tfc96_MaxNumberOfTFC_DL [enum=4]

maxNumberOfTF: tf64_MaxNumberOfTF [enum=1]

ul_TransChCapability:

maxNoBitsTransmitted: b3840_MaxNoBits [enum=3]

maxConvCodeBitsTransmitted: b1280_MaxNoBits [enum=1]

turboEncodingSupport:

supported: b3840_MaxNoBits [enum=3]

maxSimultaneousTransChs: e8_MaxSimultaneousTransChsUL [enum=2]

modeSpecificInfo:

fdd: NULL

maxTransmittedBlocks: tb8_MaxTransportBlocksUL [enum=2]

maxNumberOfTFC: tfc32_MaxNumberOfTFC_UL [enum=3]

maxNumberOfTF: tf32_MaxNumberOfTF [enum=0]

rf_Capability:

fddRF_Capability:

ue_PowerClass: 4

txRxFrequencySeparation: mhz190_TxRxFrequencySeparation [enum=0]

tddRF_Capability: Omitted

physicalChannelCapability:

fddPhysChCapability:

downlinkPhysChCapability:

maxNoDPCH_PDSCH_Codes: 3

maxNoPhysChBitsReceived: b9600_MaxNoPhysChBitsReceived [enum=6]

supportForSF_512: 0

supportOfPDSCH: 0

simultaneousSCCPCH_DPCH_Reception:

notSupported: NULL

uplinkPhysChCapability:

maxNoDPDCH_BitsTransmitted: b2400_MaxNoDPDCH_BitsTransmitted [enum=2]

supportOfPCPCH: 0

tddPhysChCapability: Omitted

ue_MultiModeRAT_Capability:

multiRAT_CapabilityList:

supportOfGSM: 0

supportOfMulticarrier: 0

multiModeCapability: fdd_MultiModeCapability [enum=1]

securityCapability:

cipheringAlgorithmCap: 0000000000000001

integrityProtectionAlgorithmCap: 0000000000000010

ue_positioning_Capability:

standaloneLocMethodsSupported: 0

ue_BasedOTDOA_Supported: 0

networkAssistedGPS_Supported: noNetworkAssistedGPS_NetworkAssistedGPS_Supported [enum=3]

supportForUE_GPS_TimingOfCellFrames: 0

supportForIPDL: 0

measurementCapability:

downlinkCompressedMode:

fdd_Measurements: 1

tdd_Measurements: Omitted

gsm_Measurements:

gsm900: 1

dcs1800: 1

gsm1900: 0

multiCarrierMeasurements: 0

uplinkCompressedMode:

fdd_Measurements: 1

tdd_Measurements: Omitted

gsm_Measurements:

gsm900: 1

dcs1800: 1

gsm1900: 0

multiCarrierMeasurements: 0

ue_RATSpecificCapability: Omitted

v370NonCriticalExtensions: Omitted

Layer 3 SDU:

[0]4A 0C 00 00 80 00 05 E2
[8]34 1A 20 90 98 CD 08 C5
[16]92 60 41 00 01 00 02 31
[24]F1 F0

#### MAC_DATA_REQ

RLC MAC @ 00:01:01.370

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 2

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 20 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:2

#### PHY_DATA_REQ

MAC PHY @ 00:01:01.370

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 2

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 02 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 20 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### RLC_AM_DATA_IND

LLA RRC @ 00:01:01.380

Channel ID: Rb2
Cell ID: -1

Message Details:

RLC_AM_DATA_IND:

cellId:-1

routingInfo:

rB_Identity:2

integrityResult:

integrityUsed (IntegrityStatus):i_pass

aM_message:

uL_DCCH_Message:

integrityCheckInfo: Omit

message: (UL_DCCH_MessageType)

rrcConnectionSetupComplete:

rrc_TransactionIdentifier:0

startList:

STARTSingle:

cn_DomainIdentity:ps_domain
start_Value:00000000000000000010

STARTSingle:

cn_DomainIdentity:cs_domain
start_Value:00000000000000000010

ue_RadioAccessCapability:

accessStratumReleaseIndicator:r99

pdcp_Capability:

losslessSRNS_RelocationSupport:true

supportForRfc2507:

supported (MaxHcContextSpace):by8192

rlc_Capability:

totalRLC_AM_BufferSize:kb50
maximumRLC_WindowSize:mws2047
maximumAM_EntityNumber (MaximumAM_EntityNumberRLC_Cap):am6

transportChannelCapability:

dl_TransChCapability:

maxNoBitsReceived (MaxNoBits):b5120
maxConvCodeBitsReceived (MaxNoBits):b1280

turboDecodingSupport: (TurboSupport)

supported (MaxNoBits):b5120

maxSimultaneousTransChs (MaxSimultaneousTransChsDL):e8
maxSimultaneousCCTrCH_Count:1
maxReceivedTransportBlocks (MaxTransportBlocksDL):tb16
maxNumberOfTFC (MaxNumberOfTFC_DL):tfc96
maxNumberOfTF:tf64

ul_TransChCapability:

maxNoBitsTransmitted (MaxNoBits):b3840
maxConvCodeBitsTransmitted (MaxNoBits):b1280

turboEncodingSupport: (TurboSupport)

supported (MaxNoBits):b3840

maxSimultaneousTransChs (MaxSimultaneousTransChsUL):e8

modeSpecificInfo:

fdd:

maxTransmittedBlocks (MaxTransportBlocksUL):tb8
maxNumberOfTFC (MaxNumberOfTFC_UL):tfc32
maxNumberOfTF:tf32

rf_Capability:

fddRF_Capability:

ue_PowerClass:4
txRxFrequencySeparation:mhz190

tddRF_Capability: Omit

physicalChannelCapability:

fddPhysChCapability:

downlinkPhysChCapability: (DL_PhysChCapabilityFDD)

maxNoDPCH_PDSCH_Codes:3
maxNoPhysChBitsReceived:b9600
supportForSF_512:false
supportOfPDSCH:false

simultaneousSCCPCH_DPCH_Reception:

notSupported:

uplinkPhysChCapability: (UL_PhysChCapabilityFDD)

maxNoDPDCH_BitsTransmitted:b2400
supportOfPCPCH:false

tddPhysChCapability: Omit

ue_MultiModeRAT_Capability:

multiRAT_CapabilityList: (MultiRAT_Capability)

supportOfGSM:false
supportOfMulticarrier:false

multiModeCapability:fdd

securityCapability:

cipheringAlgorithmCap:0000000000000001
integrityProtectionAlgorithmCap:0000000000000010

ue_positioning_Capability:

standaloneLocMethodsSupported:false
ue_BasedOTDOA_Supported:false
networkAssistedGPS_Supported:noNetworkAssistedGPS
supportForUE_GPS_TimingOfCellFrames:false
supportForIPDL:false

measurementCapability:

downlinkCompressedMode: (CompressedModeMeasCapability)

fdd_Measurements:true
tdd_Measurements: Omit

gsm_Measurements:

gsm900:true
dcs1800:true
gsm1900:false

multiCarrierMeasurements:false

uplinkCompressedMode: (CompressedModeMeasCapability)

fdd_Measurements:true
tdd_Measurements: Omit

gsm_Measurements:

gsm900:true
dcs1800:true
gsm1900:false

multiCarrierMeasurements:false

ue_RATSpecificCapability: (InterRAT_UE_RadioAccessCapabilityList) Omit

v370NonCriticalExtensions: Omit

#### RLC_AM_DATA_IND: initialDirectTransfer

RLC RRC @ 00:01:01.370

Channel No: 3 Name: DCCH

Message Details:

UL_DCCH_Message:

integrityCheckInfo: Omitted

message:

initialDirectTransfer:

cn_DomainIdentity: ps_domain_CN_DomainIdentity [enum=1]

intraDomainNasNodeSelector:

version:

release99:

cn_Type:

gsm_Map_IDNNS:

routingbasis:

localPTMSI:

routingparameter: 0011010001

enteredparameter: 0

nas_Message: 080C0005F41234567832020000

measuredResultsOnRACH: Omitted

v3a0NonCriticalExtensions:

initialDirectTransfer_v3a0ext:

start_Value: 00000000000000000010

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]15 80 D1 00 60 40 60 00
[8]2F A0 91 A2 B3 C1 90 10
[16]00 02 00 00 40

#### RRC_DATA_IND: gmm:serviceRequest

RRC NAS @ 00:01:01.370

Cell ID: -1

Message Details:

SERVICEREQUEST:

skipIndicator: 0000

gMMProtocolDiscriminator: 1000

msgType: 00001100

serviceType:

spare1: 0

type: 000

ciphKeySeqNo:

spare1: 0

keySeq: 000

ptmsi:

iel: 05

iDigit1: 1111

oddEvenInd: 0

typeOfId: 100

otherDigits: 12345678

pDP_ContextStatus:

iei: 00110010

iel: 02

nSAPI: 0000000000000000

#### RRC_DATA_REQ: gmm:authenticationAndCipheringRequest

NAS RRC @ 00:01:01.400

Cell ID: -1

Message Details:

AUTHENTICATIONANDCIPHERINGREQUEST:

skipIndicator: 0000

gMMProtocolDiscriminator: 1000

msgType: 00010010

imeisvReq:

spare1: 0

value: 000

ciphAlgorithm:

spare1: 0

algorithm: 001

acRefNo:

value: 0011

forceToStandby:

spare: 0

value: 000

authRand:

iei: 00100001

randValue: 01010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101010101

gprsCiphKeySeqNo:

iei: 1000

spare1: 0

keySeq: 001

aUTN:

iei: 00101000

iel: 10

aUTN: 01100110000100010000000000110011001000101101110100000000000000000101010101000100011101110110011000010001000000000011001100100010

#### RLC_AM_DATA_REQ:downlinkDirectTransfer

RRC RLC @ 00:01:01.400

Channel No: 3 Name: DCCH

Message Details:

Opt1: 0

Opt2: 0

DL_DCCH_Message:

integrityCheckInfo: Omitted

message:

downlinkDirectTransfer:

r3:

downlinkDirectTransfer_r3:

rrc_TransactionIdentifier: 0

cn_DomainIdentity: ps_domain_CN_DomainIdentity [enum=1]

nas_Message: 0812013021555555555555555555555555555555558128106611003322DD00005544776611003322

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]14 20 4E 10 24 02 60 42
[8]AA AA AA AA AA AA AA AA
[16]AA AA AA AA AA AA AA AB
[24]02 50 20 CC 22 00 66 45
[32]BA 00 00 AA 88 EE CC 22
[40]00 66 44

#### MAC_DATA_REQ

RLC MAC @ 00:01:01.510

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 16

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 00 14 20 4E 10 24 02
[8]60 42 AA AA AA AA AA AA
[16]AA AA

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:0
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]14 20 4E 10 24 02 60 42
[8]AA AA AA AA AA AA AA AA

#### MAC_DATA_REQ

RLC MAC @ 00:01:01.510

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 16

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 08 AA AA AA AA AA AA
[8]AA AB 02 50 20 CC 22 00
[16]66 45

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:1
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]AA AA AA AA AA AA AA AB
[8]02 50 20 CC 22 00 66 45

#### MAC_DATA_REQ

RLC MAC @ 00:01:01.510

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 16

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 15 17 FE BA 00 00 AA
[8]88 EE CC 22 00 66 44 00
[16]00 00

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:2
Polling bit:1 (request a status report)
Length indicator 0 (octets):11
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (11 octets):

[0]BA 00 00 AA 88 EE CC 22
[8]00 66 44
Padding associated with length indicator 1 (3 octets):

[0]00 00 00

#### PHY_DATA_REQ

MAC PHY @ 00:01:01.510

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 16

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 00 01 42 04 E1 02 40
[8]26 04 2A AA AA AA AA AA
[16]AA AA A0 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 00 14 20 4E 10 24 02
[8]60 42 AA AA AA AA AA AA
[16]AA AA

#### PHY_DATA_REQ

MAC PHY @ 00:01:01.520

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 17

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 00 8A AA AA AA AA AA
[8]AA AA B0 25 02 0C C2 20
[16]06 64 50 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 08 AA AA AA AA AA AA
[8]AA AB 02 50 20 CC 22 00
[16]66 45

#### PHY_DATA_REQ

MAC PHY @ 00:01:01.530

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 18

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 01 51 7F EB A0 00 0A
[8]A8 8E EC C2 20 06 64 40
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 15 17 FE BA 00 00 AA
[8]88 EE CC 22 00 66 44 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:01:01.540

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 255

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 00 D1 5F E9 26 04 10
[8]00 10 00 23 1F 1F 05 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 0D 15 FE 92 60 41 00
[8]01 00 02 31 F1 F0 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:01:01.540

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 255

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 0D 15 FE 92 60 41 00
[8]01 00 02 31 F1 F0 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:1
Polling bit:1 (request a status report)
Length indicator 0 (octets):10
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (10 octets):

[0]92 60 41 00 01 00 02 31
[8]F1 F0
Padding associated with length indicator 1 (4 octets):

[0]55 55 55 55

#### MAC_DATA_REQ

RLC MAC @ 00:01:01.550

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 20

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 20 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:2

#### PHY_DATA_REQ

MAC PHY @ 00:01:01.550

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 20

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]10 20 02 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]02 00 20 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:01:01.560

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 1

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 00 D0 BF E0 00 20 00
[8]04 05 55 55 55 55 55 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 0D 0B FE 00 02 00 00
[8]40 55 55 55 55 55 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:01:01.560

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 1

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 0D 0B FE 00 02 00 00
[8]40 55 55 55 55 55 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:1
Polling bit:1 (request a status report)
Length indicator 0 (octets):5
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (5 octets):

[0]00 02 00 00 40
Padding associated with length indicator 1 (9 octets):

[0]55 55 55 55 55 55 55 55
[8]55

#### MAC_DATA_REQ

RLC MAC @ 00:01:01.570

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 22

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 20 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:2

#### PHY_DATA_REQ

MAC PHY @ 00:01:01.570

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 22

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 02 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 20 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### MAC_DATA_REQ

RLC MAC @ 00:01:01.710

Category: Configuration
BTS unit: 1:
Channel No: 3 Name: DCCH
CFN: 36

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 15 17 FE BA 00 00 AA
[8]88 EE CC 22 00 66 44 00
[16]00 00

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:2
Polling bit:1 (request a status report)
Length indicator 0 (octets):11
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (11 octets):

[0]BA 00 00 AA 88 EE CC 22
[8]00 66 44
Padding associated with length indicator 1 (3 octets):

[0]00 00 00

#### PHY_DATA_REQ

MAC PHY @ 00:01:01.710

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 36

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 01 51 7F EB A0 00 0A
[8]A8 8E EC C2 20 06 64 40
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 15 17 FE BA 00 00 AA
[8]88 EE CC 22 00 66 44 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:01:01.770

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 22

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 03 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### MAC_DATA_IND

MAC RLC @ 00:01:01.770

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 22

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:3

#### PHY_DATA_IND

PHY MAC @ 00:01:01.910

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 36

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 01 06 C8 0A 84 09 81
[8]91 2A A2 3B B3 14 86 08
[16]80 19 90 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 10 6C 80 A8 40 98 19
[8]12 AA 23 BB 31 48 60 88
[16]01 99

#### MAC_DATA_IND

MAC RLC @ 00:01:01.910

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 36

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 10 6C 80 A8 40 98 19
[8]12 AA 23 BB 31 48 60 88
[16]01 99

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:2
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]6C 80 A8 40 98 19 12 AA
[8]23 BB 31 48 60 88 01 99

#### PHY_DATA_IND

PHY MAC @ 00:01:01.920

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 37

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 01 D1 3F E1 6E E6 7F
[8]F7 4C C4 5D D5 05 55 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 1D 13 FE 16 EE 67 FF
[8]74 CC 45 DD 50 55 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:01:01.920

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 37

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 1D 13 FE 16 EE 67 FF
[8]74 CC 45 DD 50 55 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:3
Polling bit:1 (request a status report)
Length indicator 0 (octets):9
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (9 octets):

[0]16 EE 67 FF 74 CC 45 DD
[8]50
Padding associated with length indicator 1 (5 octets):

[0]55 55 55 55 55

#### RLC_AM_DATA_IND: uplinkDirectTransfer

RLC RRC @ 00:01:01.930

Channel No: 3 Name: DCCH

Message Details:

UL_DCCH_Message:

integrityCheckInfo: Omitted

message:

uplinkDirectTransfer:

cn_DomainIdentity: ps_domain_CN_DomainIdentity [enum=1]

nas_Message: 0813032255447766290C11003322DDCCFFEE9988BBAA

measuredResultsOnRACH: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]6C 80 A8 40 98 19 12 AA
[8]23 BB 31 48 60 88 01 99
[16]16 EE 67 FF 74 CC 45 DD
[24]50

#### RRC_DATA_IND: gmm:authenticationAndCipheringResponse

RRC NAS @ 00:01:01.930

Cell ID: -1

Message Details:

AUTHENTICATIONANDCIPHERINGRESPONSE:

skipIndicator: 0000

gMMProtocolDiscriminator: 1000

msgType: 00010011

spare4: 0000

acRefNo:

value: 0011

authRsp:

iei: 00100010

value: 01010101010001000111011101100110

imeisv: Omitted

authRspExt:

iei: 00101001

iel: 0C

rES: 000100010000000000110011001000101101110111001100111111111110111010011001100010001011101110101010

#### MAC_DATA_REQ

RLC MAC @ 00:01:01.930

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 58

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 40 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:4

#### PHY_DATA_REQ

MAC PHY @ 00:01:01.930

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 58

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 04 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 40 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### CRLC_SecurityMode_Config_REQ

RRC LLA @ 00:01:01.960

Cell ID: -1

Message Details:

CRLC_SecurityMode_Config_REQ:

cellId:-1

rlcSecurityInfo: (SecurityInfo)

cn_DomainIdentity:ps_domain
startValue (START_Value):00000000000000000000
cipheringKey: Omit
integrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
gsmCipheringKey: Omit

#### CRLC_SecurityMode_Config_REQ

RRC RLC @ 00:01:01.960

Message Details:

cellIdentity: 1

rlcSecurityInfo:

cn_DomainIdentity: ps_domain_CN_DomainIdentity

startValue: 00000000000000000000

cipheringKey: Omitted

integrityKey: 01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100

#### PHY_DATA_IND

PHY MAC @ 00:01:01.970

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 42

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 03 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### MAC_DATA_IND

MAC RLC @ 00:01:01.970

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 42

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:3

#### CRLC_SecurityMode_Config_CNF

LLA RRC @ 00:01:01.970

Cell ID: -1

Message Details:

CRLC_SecurityMode_Config_CNF:

cellId:-1

#### CRLC_SetRRC_MessageSN_REQ

RRC LLA @ 00:01:01.970

Channel ID: Rb0
Cell ID: 0

Message Details:

CRLC_SetRRC_MessageSN_REQ:

cellId:0

routingInfo:

rB_Identity:0

count_I_LSB_UL (RRC_SequenceNumber): Omit
count_I_LSB_DL (RRC_SequenceNumber):0

#### CRLC_SetRRC_MessageSN_CNF

LLA RRC @ 00:01:01.990

Channel ID: Rb0
Cell ID: 0

Message Details:

CRLC_SetRRC_MessageSN_CNF:

cellId:0

routingInfo:

rB_Identity:0

#### CRLC_SetRRC_MessageSN_REQ

RRC LLA @ 00:01:01.990

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_REQ:

cellId:-1

routingInfo:

rB_Identity:1

count_I_LSB_UL (RRC_SequenceNumber): Omit
count_I_LSB_DL (RRC_SequenceNumber):0

#### CRLC_SetRRC_MessageSN_CNF

LLA RRC @ 00:01:02.010

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_CNF:

cellId:-1

routingInfo:

rB_Identity:1

#### CRLC_SetRRC_MessageSN_REQ

RRC LLA @ 00:01:02.010

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_REQ:

cellId:-1

routingInfo:

rB_Identity:2

count_I_LSB_UL (RRC_SequenceNumber): Omit
count_I_LSB_DL (RRC_SequenceNumber):0

#### CRLC_SetRRC_MessageSN_CNF

LLA RRC @ 00:01:02.020

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_CNF:

cellId:-1

routingInfo:

rB_Identity:2

#### CRLC_SetRRC_MessageSN_REQ

RRC LLA @ 00:01:02.020

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_REQ:

cellId:-1

routingInfo:

rB_Identity:3

count_I_LSB_UL (RRC_SequenceNumber): Omit
count_I_LSB_DL (RRC_SequenceNumber):0

#### CRLC_SetRRC_MessageSN_CNF

LLA RRC @ 00:01:02.040

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_CNF:

cellId:-1

routingInfo:

rB_Identity:3

#### CRLC_SetRRC_MessageSN_REQ

RRC LLA @ 00:01:02.040

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_REQ:

cellId:-1

routingInfo:

rB_Identity:4

count_I_LSB_UL (RRC_SequenceNumber): Omit
count_I_LSB_DL (RRC_SequenceNumber):0

#### CRLC_SetRRC_MessageSN_CNF

LLA RRC @ 00:01:02.050

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_SetRRC_MessageSN_CNF:

cellId:-1

routingInfo:

rB_Identity:4

#### CRLC_Integrity_Activate_REQ

RRC LLA @ 00:01:02.050

Cell ID: -1

Message Details:

CRLC_Integrity_Activate_REQ:

cellId:-1
cn_DomainIdentity:ps_domain

integrityActivationInfo:

integrityProtectionModeInfo:

integrityProtectionModeCommand:

startIntegrityProtection:

integrityProtInitNumber:00001111000011110000111100001111

integrityProtectionAlgorithm:uia1

#### CRLC_Integrity_Activate_REQ

RRC RLC @ 00:01:02.050

Message Details:

cellIdentity: 1

integrityActivationInfo:

integrityProtectionModeInfo:

integrityProtectionModeCommand:

startIntegrityProtection:

integrityProtInitNumber: 00001111000011110000111100001111

#### CRLC_Integrity_Activate_CNF

LLA RRC @ 00:01:02.070

Cell ID: -1

Message Details:

CRLC_Integrity_Activate_CNF:

cellId:-1

#### CRLC_Integrity_Activate_REQ

RRC LLA @ 00:01:02.070

Cell ID: -1

Message Details:

CRLC_Integrity_Activate_REQ:

cellId:-1
cn_DomainIdentity:ps_domain

integrityActivationInfo:

ul_IntegProtActivationInfo: (IntegrityProtActivationInfoList)

SS_IntegrityProtActivationTimeInfo:

rb_Identity:2
rrc_MessageSequenceNumber:0

#### CMAC Integrity Check Request

RRC MAC @ 00:01:02.080

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000001
Data:

[0]00 00 00 01
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:1 (RNC to UE)
Message Length (bits):120
Message:

[0]80 00 00 01 04 04 00 00
[8]80 01 41 E1 E1 E1 F0

#### CMAC Integrity Check Result

MAC RRC @ 00:01:02.080

Message Details:

Integrity Check Result:

MAC-I:00101001110000010111010101011011
Data:

[0]29 C1 75 5B

#### CRLC_Integrity_Activate_CNF

LLA RRC @ 00:01:02.080

Cell ID: -1

Message Details:

CRLC_Integrity_Activate_CNF:

cellId:-1

#### RLC_AM_DATA_REQ

RRC LLA @ 00:01:02.080

Channel ID: Rb2
Cell ID: -1

Message Details:

RLC_AM_DATA_REQ:

cellId:-1

routingInfo:

rB_Identity:2

confirmationRequest: (AmConfirmationRequest)

noConfirmationRequest:

aM_message:

dL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode:00000000000000000000000000000000
rrc_MessageSequenceNumber:0

message: (DL_DCCH_MessageType)

securityModeCommand:

r3:

securityModeCommand_r3: (SecurityModeCommand_r3_IEs)

rrc_TransactionIdentifier:0

securityCapability:

cipheringAlgorithmCap:0000000000000001
integrityProtectionAlgorithmCap:0000000000000010

cipheringModeInfo: Omit

integrityProtectionModeInfo:

integrityProtectionModeCommand:

startIntegrityProtection:

integrityProtInitNumber:00001111000011110000111100001111

integrityProtectionAlgorithm:uia1

cn_DomainIdentity:ps_domain

ue_SystemSpecificSecurityCap: (InterRAT_UE_SecurityCapList) Omit

laterNonCriticalExtensions: Omit

#### RLC_AM_DATA_REQ: securityModeCommand

LLA RLC @ 00:01:02.080

Channel No: 2 Name: DCCH

Message Details:

DL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode: 00101001110000010111010101011011

rrc_MessageSequenceNumber: 1

message:

securityModeCommand:

r3:

securityModeCommand_r3:

rrc_TransactionIdentifier: 0

securityCapability:

cipheringAlgorithmCap: 0000000000000001

integrityProtectionAlgorithmCap: 0000000000000010

cipheringModeInfo: Omitted

integrityProtectionModeInfo:

integrityProtectionModeCommand:

startIntegrityProtection:

integrityProtInitNumber: 00001111000011110000111100001111

integrityProtectionAlgorithm: uia1_IntegrityProtectionAlgorithm [enum=0]

cn_DomainIdentity: ps_domain_CN_DomainIdentity [enum=1]

ue_SystemSpecificSecurityCap: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]94 E0 BA AD 8C 04 00 00
[8]80 01 41 E1 E1 E1 F0

#### PHY_DATA_IND

PHY MAC @ 00:01:02.120

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 57

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 01 D1 3F E1 6E E6 7F
[8]F7 4C C4 5D D5 05 55 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 1D 13 FE 16 EE 67 FF
[8]74 CC 45 DD 50 55 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:01:02.120

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 57

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 1D 13 FE 16 EE 67 FF
[8]74 CC 45 DD 50 55 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:3
Polling bit:1 (request a status report)
Length indicator 0 (octets):9
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (9 octets):

[0]16 EE 67 FF 74 CC 45 DD
[8]50
Padding associated with length indicator 1 (5 octets):

[0]55 55 55 55 55

#### MAC_DATA_REQ

RLC MAC @ 00:01:02.130

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 78

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 40 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:4

#### PHY_DATA_REQ

MAC PHY @ 00:01:02.130

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 78

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 04 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 40 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### MAC_DATA_REQ

RLC MAC @ 00:01:02.150

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 80

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 05 1E 94 E0 BA AD 8C
[8]04 00 00 80 01 41 E1 E1
[16]E1 F0

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:0
Polling bit:1 (request a status report)
Length indicator 0 (octets):15
Segment associated with length indicator 0 (15 octets):

[0]94 E0 BA AD 8C 04 00 00
[8]80 01 41 E1 E1 E1 F0

#### PHY_DATA_REQ

MAC PHY @ 00:01:02.150

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 80

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 00 51 E9 4E 0B AA D8
[8]C0 40 00 08 00 14 1E 1E
[16]1E 1F 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 05 1E 94 E0 BA AD 8C
[8]04 00 00 80 01 41 E1 E1
[16]E1 F0

#### MAC_DATA_REQ

RLC MAC @ 00:01:02.350

Category: Configuration
BTS unit: 1:
Channel No: 2 Name: DCCH
CFN: 100

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 05 1E 94 E0 BA AD 8C
[8]04 00 00 80 01 41 E1 E1
[16]E1 F0

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:0
Polling bit:1 (request a status report)
Length indicator 0 (octets):15
Segment associated with length indicator 0 (15 octets):

[0]94 E0 BA AD 8C 04 00 00
[8]80 01 41 E1 E1 E1 F0

#### PHY_DATA_REQ

MAC PHY @ 00:01:02.350

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 100

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 00 51 E9 4E 0B AA D8
[8]C0 40 00 08 00 14 1E 1E
[16]1E 1F 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 05 1E 94 E0 BA AD 8C
[8]04 00 00 80 01 41 E1 E1
[16]E1 F0

#### PHY_DATA_IND

PHY MAC @ 00:01:02.390

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 84

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]10 20 01 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]02 00 10 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### MAC_DATA_IND

MAC RLC @ 00:01:02.390

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 84

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 10 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:1

#### PHY_DATA_IND

PHY MAC @ 00:01:02.400

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 85

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 01 51 3F EC 59 1B E7
[8]10 D2 10 00 00 05 55 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 15 13 FE C5 91 BE 71
[8]0D 21 00 00 00 55 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:01:02.400

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 85

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 15 13 FE C5 91 BE 71
[8]0D 21 00 00 00 55 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:2
Polling bit:1 (request a status report)
Length indicator 0 (octets):9
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (9 octets):

[0]C5 91 BE 71 0D 21 00 00
[8]00
Padding associated with length indicator 1 (5 octets):

[0]55 55 55 55 55

#### MAC_DATA_REQ

RLC MAC @ 00:01:02.410

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 106

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:3

#### PHY_DATA_REQ

MAC PHY @ 00:01:02.410

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 106

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]10 20 03 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:01:02.410

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 86

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 02 0C CF C2 4F D8 EC
[8]80 F8 52 08 28 18 58 DA
[16]00 FB 50 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 20 CC FC 24 FD 8E C8
[8]0F 85 20 82 81 85 8D A0
[16]0F B5

#### MAC_DATA_IND

MAC RLC @ 00:01:02.410

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 86

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 20 CC FC 24 FD 8E C8
[8]0F 85 20 82 81 85 8D A0
[16]0F B5

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:4
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]CC FC 24 FD 8E C8 0F 85
[8]20 82 81 85 8D A0 0F B5

#### PHY_DATA_IND

PHY MAC @ 00:01:02.420

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 87

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 02 81 02 02 03 A0 18
[8]00 00 30 09 0E 40 08 0A
[16]81 40 30 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 28 10 20 20 3A 01 80
[8]00 03 00 90 E4 00 80 A8
[16]14 03

#### MAC_DATA_IND

MAC RLC @ 00:01:02.420

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 87

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 28 10 20 20 3A 01 80
[8]00 03 00 90 E4 00 80 A8
[16]14 03

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:5
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]10 20 20 3A 01 80 00 03
[8]00 90 E4 00 80 A8 14 03

#### PHY_DATA_IND

PHY MAC @ 00:01:02.430

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 88

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 03 51 1F E8 32 0A 12
[8]1A 22 2A 30 05 55 55 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 35 11 FE 83 20 A1 21
[8]A2 22 A3 00 55 55 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:01:02.430

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 88

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 35 11 FE 83 20 A1 21
[8]A2 22 A3 00 55 55 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:6
Polling bit:1 (request a status report)
Length indicator 0 (octets):8
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (8 octets):

[0]83 20 A1 21 A2 22 A3 00
Padding associated with length indicator 1 (6 octets):

[0]55 55 55 55 55 55

#### CMAC Integrity Check Request

RRC MAC @ 00:01:02.440

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000001
Data:

[0]00 00 00 01
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:0 (UE to RNC)
Message Length (bits):72
Message:

[0]80 00 00 01 05 21 00 00
[8]00

#### RLC_AM_DATA_IND: securityModeComplete

RLC LLA @ 00:01:02.440

Channel No: 2 Name: DCCH

Message Details:

UL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode: 10001011001000110111110011100010

rrc_MessageSequenceNumber: 1

message:

securityModeComplete:

rrc_TransactionIdentifier: 0

ul_IntegProtActivationInfo:

rrc_MessageSequenceNumberList:

RRC_MessageSequenceNumberList.element: 0

RRC_MessageSequenceNumberList.element: 0

RRC_MessageSequenceNumberList.element: 0

RRC_MessageSequenceNumberList.element: 0

RRC_MessageSequenceNumberList.element: 0

rb_UL_CiphActivationTimeInfo: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]C5 91 BE 71 0D 21 00 00
[8]00

#### CMAC Integrity Check Result

MAC RRC @ 00:01:02.440

Message Details:

Integrity Check Result:

MAC-I:10001011001000110111110011100010
Data:

[0]8B 23 7C E2

#### RLC_AM_DATA_IND

LLA RRC @ 00:01:02.440

Channel ID: Rb2
Cell ID: -1

Message Details:

RLC_AM_DATA_IND:

cellId:-1

routingInfo:

rB_Identity:2

integrityResult:

integrityUsed (IntegrityStatus):i_pass

aM_message:

uL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode:10001011001000110111110011100010
rrc_MessageSequenceNumber:1

message: (UL_DCCH_MessageType)

securityModeComplete:

rrc_TransactionIdentifier:0

ul_IntegProtActivationInfo: (IntegrityProtActivationInfo)

rrc_MessageSequenceNumberList:

RRC_MessageSequenceNumber:0
RRC_MessageSequenceNumber:0
RRC_MessageSequenceNumber:0
RRC_MessageSequenceNumber:0
RRC_MessageSequenceNumber:0

rb_UL_CiphActivationTimeInfo: (RB_ActivationTimeInfoList) Omit

laterNonCriticalExtensions: Omit

#### CRLC_Integrity_Activate_REQ

RRC LLA @ 00:01:02.440

Cell ID: -1

Message Details:

CRLC_Integrity_Activate_REQ:

cellId:-1
cn_DomainIdentity:ps_domain

integrityActivationInfo:

ul_IntegProtActivationInfo: (IntegrityProtActivationInfoList)

SS_IntegrityProtActivationTimeInfo:

rb_Identity:0
rrc_MessageSequenceNumber:0

SS_IntegrityProtActivationTimeInfo:

rb_Identity:1
rrc_MessageSequenceNumber:0

SS_IntegrityProtActivationTimeInfo:

rb_Identity:3
rrc_MessageSequenceNumber:0

SS_IntegrityProtActivationTimeInfo:

rb_Identity:4
rrc_MessageSequenceNumber:0

#### RLC_AM_DATA_IND: uplinkDirectTransfer

RLC RRC @ 00:01:02.440

Channel No: 3 Name: DCCH

Message Details:

UL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode: 10011001111110000100100111111011

rrc_MessageSequenceNumber: 1

message:

uplinkDirectTransfer:

cn_DomainIdentity: ps_domain_CN_DomainIdentity [enum=1]

nas_Message: 0A4105030B1B401F6A20404074030000060121C8010150280706414243444546

measuredResultsOnRACH: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]CC FC 24 FD 8E C8 0F 85
[8]20 82 81 85 8D A0 0F B5
[16]10 20 20 3A 01 80 00 03
[24]00 90 E4 00 80 A8 14 03
[32]83 20 A1 21 A2 22 A3 00

#### RRC_DATA_IND: sm:activatePdpContextRequest

RRC NAS @ 00:01:02.440

Cell ID: -1

Message Details:

ACTIVATEPDPCONTEXTREQUESTul:

ti:

tiFlag: 0

tiVal: 000

sM_ProtocolDiscriminator: 1010

msgType: 01000001

requestedNSAPI:

spare: 0000

nSAPI_Value: 0101

requestedLLC_SAPI:

spare: 0000

nSAPI_Value: 0011

requestedQoS:

length: 0B

spare: 00

dlyClass: 011

relabilityClass: 011

peakThroughput: 0100

spare1: 0

precedenceClass: 000

spare2: 000

meanThroughput: 11111

trafficClass: 011

deliveryOrder: 01

deliveryErrorSDU: 010

maxSDUSize: 20

maxBitRateUplink: 40

maxBitRateDnlink: 40

residualBER: 0111

sduErrRatio: 0100

transDly: 000000

trafficHandpro: 11

bitRateUplink: 00

bitRateDnlink: 00

pDP_Address:

length: 06

spare: 0000

pDP_TypeOrg: 0001

pDP_TypeNo: 21

addrInfo: C8010150

accessPtName:

iei: 00101000

length: 07

accessPtName: 06414243444546

protocolConfOpts: Omitted

#### MAC_DATA_REQ

RLC MAC @ 00:01:02.440

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 109

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 70 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:7

#### PHY_DATA_REQ

MAC PHY @ 00:01:02.440

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 109

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 07 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 70 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### CMAC Integrity Check Request

RRC MAC @ 00:01:02.460

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000001
Data:

[0]00 00 00 01
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:0 (UE to RNC)
Message Length (bits):320
Message:

[0]80 00 00 01 86 C8 0F 85
[8]20 82 81 85 8D A0 0F B5
[16]10 20 20 3A 01 80 00 03
[24]00 90 E4 00 80 A8 14 03
[32]83 20 A1 21 A2 22 A3 00

#### CMAC Integrity Check Result

MAC RRC @ 00:01:02.460

Message Details:

Integrity Check Result:

MAC-I:10011001111110000100100111111011
Data:

[0]99 F8 49 FB

#### CRLC_Integrity_Activate_CNF

LLA RRC @ 00:01:02.460

Cell ID: -1

Message Details:

CRLC_Integrity_Activate_CNF:

cellId:-1

#### CPHY_Frame_Number_REQ

RRC LLA @ 00:01:02.470

Channel ID: DL-DPCH#1
Cell ID: 0

Message Details:

CPHY_Frame_Number_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:26

#### CPHY BTS Monitor & SFN CNF

PHY RRC @ 00:01:02.490

BTS unit: 1:1
CFN: 114

Message Details:

SFN:114
Tx Attenuation in dB:5
Rx Ref Power in dBm:0
TxP_SCH in dBm:-45
TxS_SCH in dBm:-45
TxP_CPICH in dBm:-40
TxP_CCPCH in dBm:-42
TxS_CCPCH in dBm:-42
TxDPSCH in dBm:-
TxPICH in dBm:-45
TxAICH in dBm:-45
TxDPCCH in dBm:-45
TxDPDCH1 in dBm:-45
TxDPDCH2 in dBm:-
TxDPDCH3 in dBm:-
TxAWGN in dBm:-
RxTotal in dBm:21.3
RxPRACH in dBm:-17.7
RxPCPCH in dBm:-
RxDPCCH in dBm:20
RxDPDCH1 in dBm:10.8
RxDPDCH2 in dBm:-
RxDPDCH3 in dBm:-
FreqError in Hz:-3
TimingError in chip:0.4

#### CPHY_Frame_Number_CNF

LLA RRC @ 00:01:02.510

Channel ID: DL-DPCH#1
Cell ID: 0

Message Details:

CPHY_Frame_Number_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:26

frameNumber:114

#### RLC_AM_DATA_REQ

RRC LLA @ 00:01:02.510

Channel ID: Rb2
Cell ID: -1

Message Details:

RLC_AM_DATA_REQ:

cellId:-1

routingInfo:

rB_Identity:2

confirmationRequest: (AmConfirmationRequest)

confirmationRequested (Mui):0

aM_message:

dL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode:00000000000000000000000000000000
rrc_MessageSequenceNumber:0

message: (DL_DCCH_MessageType)

radioBearerSetup:

r3:

radioBearerSetup_r3: (RadioBearerSetup_r3_IEs)

rrc_TransactionIdentifier:0

integrityProtectionModeInfo: Omit

cipheringModeInfo: Omit

activationTime:104

new_U_RNTI: (U_RNTI) Omit

new_C_RNTI (C_RNTI): Omit
rrc_StateIndicator:cell_DCH
utran_DRX_CycleLengthCoeff (UTRAN_DRX_CycleLengthCoefficient): Omit
ura_Identity: Omit

cn_InformationInfo: Omit

srb_InformationSetupList: Omit

rab_InformationSetupList:

RAB_InformationSetup:

rab_Info:

rab_Identity:

gsm_MAP_RAB_Identity:00000101

cn_DomainIdentity:ps_domain
nas_Synchronisation_Indicator: Omit
re_EstablishmentTimer:useT315

rb_InformationSetupList:

RB_InformationSetup:

rb_Identity:20

pdcp_Info:

losslessSRNS_RelocSupport:

notSupported:

pdcp_PDU_Header:absent

headerCompressionInfoList: Omit

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw128
timerRST:tr500
max_RST (MaxRST):rst4

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw128

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

rb_MappingInfo:

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

dch (TransportChannelIdentity):1

logicalChannelIdentity: Omit

rlc_SizeList:

configured:

mac_LogicalChannelPriority:8

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

dch (TransportChannelIdentity):6

logicalChannelIdentity: Omit

RB_MappingOption:

ul_LogicalChannelMappings:

oneLogicalChannel: (UL_LogicalChannelMapping)

ul_TransportChannelType:

rach:

logicalChannelIdentity:7

rlc_SizeList:

explicitList: (RLC_SizeExplicitList)

RLC_SizeInfo:

rlc_SizeIndex:2

mac_LogicalChannelPriority:8

dl_LogicalChannelMappingList:

DL_LogicalChannelMapping:

dl_TransportChannelType:

fach:

logicalChannelIdentity:7

rb_InformationAffectedList: Omit

dl_CounterSynchronisationInfo: Omit

ul_CommonTransChInfo:

tfc_Subset: Omit

prach_TFCS: (TFCS) Omit

modeSpecificInfo:

fdd:

ul_TFCS: (TFCS)

normalTFCI_Signalling: (ExplicitTFCS_Configuration)

complete: (TFCS_ReconfAdd)

ctfcSize:

ctfc4Bit:

:

ctfc4:0

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:1

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:2

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:3

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:4

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:5

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:6

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:7

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:8

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:9

powerOffsetInformation:

gainFactorInformation:

signalledGainFactors:

modeSpecificInfo:

fdd:

gainFactorBetaC (GainFactor):9

gainFactorBetaD (GainFactor):15
referenceTFC_ID:0

powerOffsetPp_m: Omit

ul_deletedTransChInfoList: Omit

ul_AddReconfTransChInfoList:

UL_AddReconfTransChInformation:

ul_TransportChannelType (UL_TrCH_Type):dch
transportChannelIdentity:1

transportFormatSet:

dedicatedTransChTFS:

tti:

tti20: (DedicatedDynamicTF_InfoList)

DedicatedDynamicTF_Info:

rlc_Size:

octetModeType1: (OctetModeRLC_SizeInfoType1)

sizeType2:

part1:2
part2: Omit

numberOfTbSizeList:

NumberOfTransportBlocks:

zero:

NumberOfTransportBlocks:

one:

NumberOfTransportBlocks:

small:2

NumberOfTransportBlocks:

small:3

NumberOfTransportBlocks:

small:4

logicalChannelList:

allSizes:

semistaticTF_Information:

channelCodingType:

turbo:

rateMatchingAttribute:150
crc_Size:crc16

UL_AddReconfTransChInformation:

ul_TransportChannelType (UL_TrCH_Type):dch
transportChannelIdentity:5

transportFormatSet:

dedicatedTransChTFS:

tti:

tti40: (DedicatedDynamicTF_InfoList)

DedicatedDynamicTF_Info:

rlc_Size:

bitMode: (BitModeRLC_SizeInfo)

sizeType2:

part1:2
part2: Omit

numberOfTbSizeList:

NumberOfTransportBlocks:

zero:

NumberOfTransportBlocks:

one:

logicalChannelList:

allSizes:

semistaticTF_Information:

channelCodingType:

convolutional (CodingRate):third

rateMatchingAttribute:170
crc_Size:crc16

modeSpecificTransChInfo:

fdd:

cpch_SetID: Omit

addReconfTransChDRAC_Info: (DRAC_StaticInformationList) Omit

dl_CommonTransChInfo:

sccpch_TFCS: (TFCS) Omit

modeSpecificInfo:

fdd:

dl_Parameters:

dl_DCH_TFCS: (TFCS)

normalTFCI_Signalling: (ExplicitTFCS_Configuration)

complete: (TFCS_ReconfAdd)

ctfcSize:

ctfc4Bit:

:

ctfc4:0

powerOffsetInformation: Omit

:

ctfc4:1

powerOffsetInformation: Omit

:

ctfc4:2

powerOffsetInformation: Omit

:

ctfc4:3

powerOffsetInformation: Omit

:

ctfc4:4

powerOffsetInformation: Omit

:

ctfc4:5

powerOffsetInformation: Omit

:

ctfc4:6

powerOffsetInformation: Omit

:

ctfc4:7

powerOffsetInformation: Omit

:

ctfc4:8

powerOffsetInformation: Omit

:

ctfc4:9

powerOffsetInformation: Omit

dl_DeletedTransChInfoList: Omit

dl_AddReconfTransChInfoList:

DL_AddReconfTransChInformation:

dl_TransportChannelType (DL_TrCH_Type):dch
dl_transportChannelIdentity (TransportChannelIdentity):6

tfs_SignallingMode:

sameAsULTrCH: (UL_TransportChannelIdentity)

ul_TransportChannelType (UL_TrCH_Type):dch
ul_TransportChannelIdentity (TransportChannelIdentity):1

dch_QualityTarget: (QualityTarget)

bler_QualityValue:-20

dummy: (TM_SignallingInfo) Omit

DL_AddReconfTransChInformation:

dl_TransportChannelType (DL_TrCH_Type):dch
dl_transportChannelIdentity (TransportChannelIdentity):10

tfs_SignallingMode:

sameAsULTrCH: (UL_TransportChannelIdentity)

ul_TransportChannelType (UL_TrCH_Type):dch
ul_TransportChannelIdentity (TransportChannelIdentity):5

dch_QualityTarget: (QualityTarget)

bler_QualityValue:-20

dummy: (TM_SignallingInfo) Omit

frequencyInfo: Omit

maxAllowedUL_TX_Power:33

ul_ChannelRequirement:

ul_DPCH_Info:

ul_DPCH_PowerControlInfo:

fdd:

dpcch_PowerOffset:-40
pc_Preamble:1
sRB_delay:7

powerControlAlgorithm:

algorithm1 (TPC_StepSizeFDD):1

modeSpecificInfo:

fdd:

scramblingCodeType:longSC
scramblingCode (UL_ScramblingCode):0
numberOfDPDCH: Omit
spreadingFactor:sf16
tfci_Existence:true
numberOfFBI_Bits: Omit
puncturingLimit:pl0_96

modeSpecificPhysChInfo:

fdd:

dl_PDSCH_Information: Omit

dl_CommonInformation:

dl_DPCH_InfoCommon:

cfnHandling:

maintain:

modeSpecificInfo:

fdd:

dl_DPCH_PowerControlInfo:

modeSpecificInfo:

fdd:

dpc_Mode:singleTPC

powerOffsetPilot_pdpdch:0

dl_rate_matching_restriction: Omit

spreadingFactorAndPilot: (SF512_AndPilot)

sfd32:

positionFixedOrFlexible:flexible
tfci_Existence:true

modeSpecificInfo:

fdd:

defaultDPCH_OffsetValue (DefaultDPCH_OffsetValueFDD): Omit

dpch_CompressedModeInfo: Omit

tx_DiversityMode:noDiversity

ssdt_Information: Omit

dl_InformationPerRL_List:

DL_InformationPerRL:

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode:100

pdsch_SHO_DCH_Info: Omit

pdsch_CodeMapping: Omit

dl_DPCH_InfoPerRL:

fdd:

pCPICH_UsageForChannelEst:mayBeUsed
dpch_FrameOffset:0

secondaryCPICH_Info: Omit

dl_ChannelisationCodeList:

DL_ChannelisationCode:

secondaryScramblingCode:1

sf_AndCodeNumber: (SF512_AndCodeNumber)

sf32:0

scramblingCodeChange: Omit

tpc_CombinationIndex:0
ssdt_CellIdentity: Omit
closedLoopTimingAdjMode: Omit

sccpch_InfoforFACH: Omit

v3a0NonCriticalExtensions:

radioBearerSetup_v3a0ext:

new_DSCH_RNTI (DSCH_RNTI): Omit

laterNonCriticalExtensions: Omit

#### CMAC Integrity Check Request

RRC MAC @ 00:01:02.520

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000010
Data:

[0]00 00 00 02
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:1 (RNC to UE)
Message Length (bits):736
Message:

[0]80 00 00 01 03 92 04 BA
[8]F1 A0 00 17 19 DB 3D 2C
[16]9D 93 4C F9 58 9C E0 07
[24]81 75 68 01 EA C4 08 13
[32]04 8A 49 26 94 4A A5 92
[40]E9 84 C9 4F 81 00 41 42
[48]20 C1 0C 45 2A C4 20 11
[56]04 47 52 C1 02 04 80 22
[64]19 0A 63 A1 21 85 81 5C
[72]4C 4A E9 A5 47 A2 00 00
[80]00 BC 48 03 C4 08 19 00
[88]00 20 60 00

#### RLC_AM_DATA_REQ: radioBearerSetup

LLA RLC @ 00:01:02.520

Channel No: 2 Name: DCCH

Message Details:

MUI: 0

DL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode: 00101100101001101110001111000110

rrc_MessageSequenceNumber: 2

message:

radioBearerSetup:

r3:

radioBearerSetup_r3:

rrc_TransactionIdentifier: 0

integrityProtectionModeInfo: Omitted

cipheringModeInfo: Omitted

activationTime: 104

new_U_RNTI: Omitted

new_C_RNTI: Omitted

rrc_StateIndicator: cell_DCH_RRC_StateIndicator [enum=0]

utran_DRX_CycleLengthCoeff: Omitted

ura_Identity: Omitted

cn_InformationInfo: Omitted

srb_InformationSetupList: Omitted

rab_InformationSetupList:

RAB_InformationSetupList.element:

rab_Info:

rab_Identity:

gsm_MAP_RAB_Identity: 00000101

cn_DomainIdentity: ps_domain_CN_DomainIdentity [enum=1]

nas_Synchronisation_Indicator: Omitted

re_EstablishmentTimer: useT315_Re_EstablishmentTimer [enum=1]

rb_InformationSetupList:

RB_InformationSetupList.element:

rb_Identity: 20

pdcp_Info:

losslessSRNS_RelocSupport:

notSupported: NULL

pdcp_PDU_Header: absent_PDCP_PDU_Header [enum=1]

headerCompressionInfoList: Omitted

rlc_InfoChoice:

rlc_Info:

ul_RLC_Mode:

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard: dat15_MaxDAT [enum=10]

transmissionWindowSize: tw128_TransmissionWindowSize [enum=5]

timerRST: tr500_TimerRST [enum=9]

max_RST: rst4_MaxRST [enum=1]

pollingInfo:

timerPollProhibit: tpp200_TimerPollProhibit [enum=19]

timerPoll: tp200_TimerPoll [enum=19]

poll_PDU: Omitted

poll_SDU: sdu1_Poll_SDU [enum=0]

lastTransmissionPDU_Poll: 1

lastRetransmissionPDU_Poll: 1

pollWindow: pw99_PollWindow [enum=7]

timerPollPeriodic: Omitted

dl_RLC_Mode:

dl_AM_RLC_Mode:

inSequenceDelivery: 1

receivingWindowSize: rw128_ReceivingWindowSize [enum=5]

dl_RLC_StatusInfo:

timerStatusProhibit: tsp200_TimerStatusProhibit [enum=19]

timerEPC: Omitted

missingPDU_Indicator: 1

timerStatusPeriodic: Omitted

rb_MappingInfo:

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

dch: 1

logicalChannelIdentity: Omitted

rlc_SizeList:

configured: NULL

mac_LogicalChannelPriority: 8

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

dch: 6

logicalChannelIdentity: Omitted

RB_MappingInfo.element:

ul_LogicalChannelMappings:

oneLogicalChannel:

ul_TransportChannelType:

rach: NULL

logicalChannelIdentity: 7

rlc_SizeList:

explicitList:

RLC_SizeExplicitList.element:

rlc_SizeIndex: 2

mac_LogicalChannelPriority: 8

dl_LogicalChannelMappingList:

DL_LogicalChannelMappingList.element:

dl_TransportChannelType:

fach: NULL

logicalChannelIdentity: 7

rb_InformationAffectedList: Omitted

dl_CounterSynchronisationInfo: Omitted

ul_CommonTransChInfo:

tfc_Subset: Omitted

prach_TFCS: Omitted

modeSpecificInfo:

fdd:

ul_TFCS:

normalTFCI_Signalling:

complete:

ctfcSize:

ctfc4Bit:

ctfc4Bit.noName:

ctfc4: 0

powerOffsetInformation:

gainFactorInformation:

computedGainFactors: 0

powerOffsetPp_m: Omitted

ctfc4Bit.noName:

ctfc4: 1

powerOffsetInformation:

gainFactorInformation:

computedGainFactors: 0

powerOffsetPp_m: Omitted

ctfc4Bit.noName:

ctfc4: 2

powerOffsetInformation:

gainFactorInformation:

computedGainFactors: 0

powerOffsetPp_m: Omitted

ctfc4Bit.noName:

ctfc4: 3

powerOffsetInformation:

gainFactorInformation:

computedGainFactors: 0

powerOffsetPp_m: Omitted

ctfc4Bit.noName:

ctfc4: 4

powerOffsetInformation:

gainFactorInformation:

computedGainFactors: 0

powerOffsetPp_m: Omitted

ctfc4Bit.noName:

ctfc4: 5

powerOffsetInformation:

gainFactorInformation:

computedGainFactors: 0

powerOffsetPp_m: Omitted

ctfc4Bit.noName:

ctfc4: 6

powerOffsetInformation:

gainFactorInformation:

computedGainFactors: 0

powerOffsetPp_m: Omitted

ctfc4Bit.noName:

ctfc4: 7

powerOffsetInformation:

gainFactorInformation:

computedGainFactors: 0

powerOffsetPp_m: Omitted

ctfc4Bit.noName:

ctfc4: 8

powerOffsetInformation:

gainFactorInformation:

computedGainFactors: 0

powerOffsetPp_m: Omitted

ctfc4Bit.noName:

ctfc4: 9

powerOffsetInformation:

gainFactorInformation:

signalledGainFactors:

modeSpecificInfo:

fdd:

gainFactorBetaC: 9

gainFactorBetaD: 15

referenceTFC_ID: 0

powerOffsetPp_m: Omitted

ul_deletedTransChInfoList: Omitted

ul_AddReconfTransChInfoList:

UL_AddReconfTransChInfoList.element:

ul_TransportChannelType: dch_UL_TrCH_Type [enum=0]

transportChannelIdentity: 1

transportFormatSet:

dedicatedTransChTFS:

tti:

tti20:

DedicatedDynamicTF_InfoList.element:

rlc_Size:

octetModeType1:

sizeType2:

part1: 2

part2: Omitted

numberOfTbSizeList:

numberOfTbSizeList.element:

zero: NULL

numberOfTbSizeList.element:

one: NULL

numberOfTbSizeList.element:

small: 2

numberOfTbSizeList.element:

small: 3

numberOfTbSizeList.element:

small: 4

logicalChannelList:

allSizes: NULL

semistaticTF_Information:

channelCodingType:

turbo: NULL

rateMatchingAttribute: 150

crc_Size: crc16_CRC_Size [enum=3]

UL_AddReconfTransChInfoList.element:

ul_TransportChannelType: dch_UL_TrCH_Type [enum=0]

transportChannelIdentity: 5

transportFormatSet:

dedicatedTransChTFS:

tti:

tti40:

DedicatedDynamicTF_InfoList.element:

rlc_Size:

bitMode:

sizeType2:

part1: 2

part2: Omitted

numberOfTbSizeList:

numberOfTbSizeList.element:

zero: NULL

numberOfTbSizeList.element:

one: NULL

logicalChannelList:

allSizes: NULL

semistaticTF_Information:

channelCodingType:

convolutional: third_CodingRate [enum=1]

rateMatchingAttribute: 170

crc_Size: crc16_CRC_Size [enum=3]

modeSpecificTransChInfo:

fdd:

cpch_SetID: Omitted

addReconfTransChDRAC_Info: Omitted

dl_CommonTransChInfo:

sccpch_TFCS: Omitted

modeSpecificInfo:

fdd:

dl_Parameters:

dl_DCH_TFCS:

normalTFCI_Signalling:

complete:

ctfcSize:

ctfc4Bit:

ctfc4Bit.noName:

ctfc4: 0

powerOffsetInformation: Omitted

ctfc4Bit.noName:

ctfc4: 1

powerOffsetInformation: Omitted

ctfc4Bit.noName:

ctfc4: 2

powerOffsetInformation: Omitted

ctfc4Bit.noName:

ctfc4: 3

powerOffsetInformation: Omitted

ctfc4Bit.noName:

ctfc4: 4

powerOffsetInformation: Omitted

ctfc4Bit.noName:

ctfc4: 5

powerOffsetInformation: Omitted

ctfc4Bit.noName:

ctfc4: 6

powerOffsetInformation: Omitted

ctfc4Bit.noName:

ctfc4: 7

powerOffsetInformation: Omitted

ctfc4Bit.noName:

ctfc4: 8

powerOffsetInformation: Omitted

ctfc4Bit.noName:

ctfc4: 9

powerOffsetInformation: Omitted

dl_DeletedTransChInfoList: Omitted

dl_AddReconfTransChInfoList:

DL_AddReconfTransChInfoList.element:

dl_TransportChannelType: dch_DL_TrCH_Type [enum=0]

dl_transportChannelIdentity: 6

tfs_SignallingMode:

sameAsULTrCH:

ul_TransportChannelType: dch_UL_TrCH_Type [enum=0]

ul_TransportChannelIdentity: 1

dch_QualityTarget:

bler_QualityValue: -20

dummy: Omitted

DL_AddReconfTransChInfoList.element:

dl_TransportChannelType: dch_DL_TrCH_Type [enum=0]

dl_transportChannelIdentity: 10

tfs_SignallingMode:

sameAsULTrCH:

ul_TransportChannelType: dch_UL_TrCH_Type [enum=0]

ul_TransportChannelIdentity: 5

dch_QualityTarget:

bler_QualityValue: -20

dummy: Omitted

frequencyInfo: Omitted

maxAllowedUL_TX_Power: 33

ul_ChannelRequirement:

ul_DPCH_Info:

ul_DPCH_PowerControlInfo:

fdd:

dpcch_PowerOffset: -40

pc_Preamble: 1

sRB_delay: 7

powerControlAlgorithm:

algorithm1: 1

modeSpecificInfo:

fdd:

scramblingCodeType: longSC_ScramblingCodeType [enum=1]

scramblingCode: 0

numberOfDPDCH: Default

spreadingFactor: sf16_SpreadingFactor [enum=2]

tfci_Existence: 1

numberOfFBI_Bits: Omitted

puncturingLimit: pl0_96_PuncturingLimit [enum=14]

modeSpecificPhysChInfo:

fdd:

dl_PDSCH_Information: Omitted

dl_CommonInformation:

dl_DPCH_InfoCommon:

cfnHandling:

maintain: NULL

modeSpecificInfo:

fdd:

dl_DPCH_PowerControlInfo:

modeSpecificInfo:

fdd:

dpc_Mode: singleTPC_DPC_Mode [enum=0]

powerOffsetPilot_pdpdch: 0

dl_rate_matching_restriction: Omitted

spreadingFactorAndPilot:

sfd32: NULL

positionFixedOrFlexible: flexible_PositionFixedOrFlexible [enum=1]

tfci_Existence: 1

modeSpecificInfo:

fdd:

defaultDPCH_OffsetValue: Omitted

dpch_CompressedModeInfo: Omitted

tx_DiversityMode: noDiversity_TX_DiversityMode [enum=0]

ssdt_Information: Omitted

dl_InformationPerRL_List:

DL_InformationPerRL_List.element:

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode: 100

pdsch_SHO_DCH_Info: Omitted

pdsch_CodeMapping: Omitted

dl_DPCH_InfoPerRL:

fdd:

pCPICH_UsageForChannelEst: mayBeUsed_PCPICH_UsageForChannelEst [enum=0]

dpch_FrameOffset: 0

secondaryCPICH_Info: Omitted

dl_ChannelisationCodeList:

DL_ChannelisationCodeList.element:

secondaryScramblingCode: 1

sf_AndCodeNumber:

sf32: 0

scramblingCodeChange: Omitted

tpc_CombinationIndex: 0

ssdt_CellIdentity: Omitted

closedLoopTimingAdjMode: Omitted

sccpch_InfoforFACH: Omitted

v3a0NonCriticalExtensions:

radioBearerSetup_v3a0ext:

new_DSCH_RNTI: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]96 53 71 E3 13 92 04 BA
[8]F1 A0 00 17 19 DB 3D 2C
[16]9D 93 4C F9 58 9C E0 07
[24]81 75 68 01 EA C4 08 13
[32]04 8A 49 26 94 4A A5 92
[40]E9 84 C9 4F 81 00 41 42
[48]20 C1 0C 45 2A C4 20 11
[56]04 47 52 C1 02 04 80 22
[64]19 0A 63 A1 21 85 81 5C
[72]4C 4A E9 A5 47 A2 00 00
[80]00 BC 48 03 C4 08 19 00
[88]00 20 60 00

#### CMAC Integrity Check Result

MAC RRC @ 00:01:02.520

Message Details:

Integrity Check Result:

MAC-I:00101100101001101110001111000110
Data:

[0]2C A6 E3 C6

#### PHY_DATA_IND

PHY MAC @ 00:01:02.590

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 104

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]10 20 01 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]02 00 10 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### MAC_DATA_IND

MAC RLC @ 00:01:02.590

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 104

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 10 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:1

#### PHY_DATA_IND

PHY MAC @ 00:01:02.600

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 105

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 01 51 3F EC 59 1B E7
[8]10 D2 10 00 00 05 55 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 15 13 FE C5 91 BE 71
[8]0D 21 00 00 00 55 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:01:02.600

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 105

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 15 13 FE C5 91 BE 71
[8]0D 21 00 00 00 55 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:2
Polling bit:1 (request a status report)
Length indicator 0 (octets):9
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (9 octets):

[0]C5 91 BE 71 0D 21 00 00
[8]00
Padding associated with length indicator 1 (5 octets):

[0]55 55 55 55 55

#### MAC_DATA_REQ

RLC MAC @ 00:01:02.610

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 126

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:3

#### PHY_DATA_REQ

MAC PHY @ 00:01:02.610

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 126

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]10 20 03 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]02 00 30 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### MAC_DATA_REQ

RLC MAC @ 00:01:02.620

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 127

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 08 96 53 71 E3 13 92
[8]04 BA F1 A0 00 17 19 DB
[16]3D 2C

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:1
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]96 53 71 E3 13 92 04 BA
[8]F1 A0 00 17 19 DB 3D 2C

#### MAC_DATA_REQ

RLC MAC @ 00:01:02.620

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 127

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 10 9D 93 4C F9 58 9C
[8]E0 07 81 75 68 01 EA C4
[16]08 13

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:2
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]9D 93 4C F9 58 9C E0 07
[8]81 75 68 01 EA C4 08 13

#### MAC_DATA_REQ

RLC MAC @ 00:01:02.620

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 127

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 18 04 8A 49 26 94 4A
[8]A5 92 E9 84 C9 4F 81 00
[16]41 42

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:3
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]04 8A 49 26 94 4A A5 92
[8]E9 84 C9 4F 81 00 41 42

#### MAC_DATA_REQ

RLC MAC @ 00:01:02.620

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 127

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 20 20 C1 0C 45 2A C4
[8]20 11 04 47 52 C1 02 04
[16]80 22

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:4
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]20 C1 0C 45 2A C4 20 11
[8]04 47 52 C1 02 04 80 22

#### MAC_DATA_REQ

RLC MAC @ 00:01:02.620

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 127

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 28 19 0A 63 A1 21 85
[8]81 5C 4C 4A E9 A5 47 A2
[16]00 00

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:5
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]19 0A 63 A1 21 85 81 5C
[8]4C 4A E9 A5 47 A2 00 00

#### MAC_DATA_REQ

RLC MAC @ 00:01:02.620

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 127

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 35 19 FE 00 BC 48 03
[8]C4 08 19 00 00 20 60 00
[16]00 00

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:6
Polling bit:1 (request a status report)
Length indicator 0 (octets):12
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (12 octets):

[0]00 BC 48 03 C4 08 19 00
[8]00 20 60 00
Padding associated with length indicator 1 (2 octets):

[0]00 00

#### PHY_DATA_REQ

MAC PHY @ 00:01:02.620

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 127

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 00 89 65 37 1E 31 39
[8]20 4B AF 1A 00 01 71 9D
[16]B3 D2 C0 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 08 96 53 71 E3 13 92
[8]04 BA F1 A0 00 17 19 DB
[16]3D 2C

#### PHY_DATA_REQ

MAC PHY @ 00:01:02.630

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 128

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 01 09 D9 34 CF 95 89
[8]CE 00 78 17 56 80 1E AC
[16]40 81 30 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 10 9D 93 4C F9 58 9C
[8]E0 07 81 75 68 01 EA C4
[16]08 13

#### PHY_DATA_IND

PHY MAC @ 00:01:02.630

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 108

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 03 51 1F E8 32 0A 12
[8]1A 22 2A 30 05 55 55 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 35 11 FE 83 20 A1 21
[8]A2 22 A3 00 55 55 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:01:02.630

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 108

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 35 11 FE 83 20 A1 21
[8]A2 22 A3 00 55 55 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:6
Polling bit:1 (request a status report)
Length indicator 0 (octets):8
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (8 octets):

[0]83 20 A1 21 A2 22 A3 00
Padding associated with length indicator 1 (6 octets):

[0]55 55 55 55 55 55

#### MAC_DATA_REQ

RLC MAC @ 00:01:02.640

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 129

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 70 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:7

#### PHY_DATA_REQ

MAC PHY @ 00:01:02.640

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 129

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 01 80 48 A4 92 69 44
[8]AA 59 2E 98 4C 94 F8 10
[16]04 14 20 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 18 04 8A 49 26 94 4A
[8]A5 92 E9 84 C9 4F 81 00
[16]41 42

#### PHY_DATA_REQ

MAC PHY @ 00:01:02.650

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 130

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 02 02 0C 10 C4 52 AC
[8]42 01 10 44 75 2C 10 20
[16]48 02 20 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 20 20 C1 0C 45 2A C4
[8]20 11 04 47 52 C1 02 04
[16]80 22

#### PHY_DATA_REQ

MAC PHY @ 00:01:02.660

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 131

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 02 81 90 A6 3A 12 18
[8]58 15 C4 C4 AE 9A 54 7A
[16]20 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 28 19 0A 63 A1 21 85
[8]81 5C 4C 4A E9 A5 47 A2
[16]00 00

#### PHY_DATA_REQ

MAC PHY @ 00:01:02.670

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 132

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 03 51 9F E0 0B C4 80
[8]3C 40 81 90 00 02 06 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 35 19 FE 00 BC 48 03
[8]C4 08 19 00 00 20 60 00
[16]00 00

#### PHY_DATA_REQ

MAC PHY @ 00:01:02.680

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 133

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 07 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 70 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### MAC_DATA_REQ

RLC MAC @ 00:01:02.820

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 147

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 35 19 FE 00 BC 48 03
[8]C4 08 19 00 00 20 60 00
[16]00 00

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:6
Polling bit:1 (request a status report)
Length indicator 0 (octets):12
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (12 octets):

[0]00 BC 48 03 C4 08 19 00
[8]00 20 60 00
Padding associated with length indicator 1 (2 octets):

[0]00 00

#### PHY_DATA_REQ

MAC PHY @ 00:01:02.820

BTS unit: 1:1
Channel No: 0 Name: DCH
CFN: 147

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 03 51 9F E0 0B C4 80
[8]3C 40 81 90 00 02 06 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 35 19 FE 00 BC 48 03
[8]C4 08 19 00 00 20 60 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:01:02.910

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 136

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]10 20 07 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]02 00 70 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### MAC_DATA_IND

MAC RLC @ 00:01:02.910

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 136

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 70 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:7

#### RLC_AM_DATA_CNF

RLC LLA @ 00:01:02.920

BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 157

Message Details:

Message Unit Identifier:0

#### RLC_AM_DATA_CNF

LLA RRC @ 00:01:02.930

Channel ID: Rb2
Cell ID: -1

Message Details:

RLC_AM_DATA_CNF:

cellId:-1

routingInfo:

rB_Identity:2

mui:0

#### CPHY_RL_Modify_REQ

RRC LLA @ 00:01:02.930

Channel ID: DL-DPCH#1
Cell ID: 0

Message Details:

CPHY_RL_Modify_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:26

ratType:fdd

modifyMessage: (CphyRlModifyReq)

activationTime: (SS_ActivationTime)

activationCFN (ActivationTime):104

physicalChannelInfo:

dPCHInfo:

ul_DPCHInfo: (UL_DPCH_Info) Omit

dl_DPCHInfo:

dl_CommonInformation:

dl_DPCH_InfoCommon:

cfnHandling:

maintain:

modeSpecificInfo:

fdd:

dl_DPCH_PowerControlInfo:

modeSpecificInfo:

fdd:

dpc_Mode:singleTPC

powerOffsetPilot_pdpdch:0

dl_rate_matching_restriction: Omit

spreadingFactorAndPilot: (SF512_AndPilot)

sfd32:

positionFixedOrFlexible:flexible
tfci_Existence:true

modeSpecificInfo:

fdd:

defaultDPCH_OffsetValue (DefaultDPCH_OffsetValueFDD): Omit

dpch_CompressedModeInfo: Omit

tx_DiversityMode:noDiversity

ssdt_Information: Omit

dl_DPCH_InfoPerRL:

fdd:

pCPICH_UsageForChannelEst:mayBeUsed
dpch_FrameOffset:0

secondaryCPICH_Info: Omit

dl_ChannelisationCodeList:

DL_ChannelisationCode:

secondaryScramblingCode:1

sf_AndCodeNumber: (SF512_AndCodeNumber)

sf32:0

scramblingCodeChange: Omit

tpc_CombinationIndex:0
ssdt_CellIdentity: Omit
closedLoopTimingAdjMode: Omit

powerOffsetOfTFCI_PO1:0
powerOffsetOfTPC_PO2:0
powerOffsetOfPILOT_PO3:0
dl_TxPower:-5
dl_TxPowerMax (DL_TxPower):15
dl_TxPowerMin (DL_TxPower):-35

#### CPHY Radio Link Setup REQ

LLA PHY @ 00:01:02.950

BTS unit: 1:1
Channel No: 0 Name: D_DPCH
CFN: 160

Message Details:

Configuration Parameters:

Activation Time:104
Channel Offset:7680
Scrambling Code:1601
Symbol Rate:120k
Channelization Code:0
Adjust Time:0
Power in dBm:-45
Tx Diversity:Off
Slot Format:13
Number Of DPDCH:1

DPDCH Parameters:

Item Number 0:

Power in dBm:-45
Channelization Code:0

#### CPHY Radio Link Setup CNF

PHY LLA @ 00:01:02.950

BTS unit: 1:1
Channel No: 0 Name: D_DPCH
CFN: 160

Message Details:

#### CPHY Transport Channel Configuration REQ

LLA PHY @ 00:01:02.990

BTS unit: 1:1
Channel No: 0 Name: D_DPCH
CFN: 164

Message Details:

Configuration Parameters:

Activation Time:104
DTX Position:Flexible
Second Interleave:On
Puncture Limit:0
CCTrCH Length:2100
Number Of Transport Channels:1

Transport Channels:

Item Number 0:

Transport Channel Parameters:

Transport Channel:

Name:D_DCH
Identity:0

TTI (ms):10
EP Type:1/3 Rate Convolutional Coding
CRC Size:16
RM Attribute:192
First Interleave:On
Number Of Transport Formats:2

Transport Format Set:

Transport Format 0:

Number Of Transport Blocks:0
Transport Block Size In Bits:148

Transport Format 1:

Number Of Transport Blocks:1
Transport Block Size In Bits:148

RM Maximum Length:2100

Transport Format Combination Set:

Number Of Transport Format Combinations:2

Transport Format Combinations 0:

Transport Format:0

Transport Format Combinations 1:

Transport Format:1

#### CPHY Transport Channel Configuration CNF

PHY LLA @ 00:01:02.990

BTS unit: 1:1
Channel No: 0 Name: D_DPCH
CFN: 164

Message Details:

#### CPHY_RL_Modify_CNF

LLA RRC @ 00:01:03.010

Channel ID: DL-DPCH#1
Cell ID: 0

Message Details:

CPHY_RL_Modify_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:26

#### CPHY_TrCH_Config_REQ

RRC LLA @ 00:01:03.010

Channel ID: DL-DPCH#1
Cell ID: 0

Message Details:

CPHY_TrCH_Config_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:26

ratType:fdd

trchConfigType:

dch:Normal

configMessage: (CphyTrchConfigReq)

activationTime: (SS_ActivationTime)

activationCFN (ActivationTime):104

ulconnectedTrCHList: Omit

ulTFCS: (TFCS) Omit

dlconnectedTrCHList:

:

trchid (TransportChannelIdentity):6
dl_TransportChannelType (SS_DL_TransportChannelType):dch

transportChannelInfo: (CommonOrDedicatedTFS)

tti:

tti20: (CommonOrDedicatedTF_InfoList)

CommonOrDedicatedTF_Info:

tb_Size:336

numberOfTbSizeList:

NumberOfTransportBlocks:

zero:

NumberOfTransportBlocks:

one:

NumberOfTransportBlocks:

small:2

NumberOfTransportBlocks:

small:3

NumberOfTransportBlocks:

small:4

logicalChannelList:

allSizes:

semistaticTF_Information:

channelCodingType:

turbo:

rateMatchingAttribute:150
crc_Size:crc16

:

trchid (TransportChannelIdentity):10
dl_TransportChannelType (SS_DL_TransportChannelType):dch

transportChannelInfo: (CommonOrDedicatedTFS)

tti:

tti40: (CommonOrDedicatedTF_InfoList)

CommonOrDedicatedTF_Info:

tb_Size:148

numberOfTbSizeList:

NumberOfTransportBlocks:

zero:

NumberOfTransportBlocks:

one:

logicalChannelList:

allSizes:

semistaticTF_Information:

channelCodingType:

convolutional (CodingRate):third

rateMatchingAttribute:170
crc_Size:crc16

dlTFCS: (TFCS)

normalTFCI_Signalling: (ExplicitTFCS_Configuration)

complete: (TFCS_ReconfAdd)

ctfcSize:

ctfc4Bit:

:

ctfc4:0

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:1

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:2

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:3

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:4

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:5

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:6

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:7

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:8

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:9

powerOffsetInformation:

gainFactorInformation:

signalledGainFactors:

modeSpecificInfo:

fdd:

gainFactorBetaC (GainFactor):9

gainFactorBetaD (GainFactor):15
referenceTFC_ID:0

powerOffsetPp_m: Omit

#### CPHY Transport Channel Configuration REQ

LLA PHY @ 00:01:03.020

BTS unit: 1:1
Channel No: 0 Name: D_DPCH
CFN: 167

Message Details:

Configuration Parameters:

Activation Time:104
DTX Position:Flexible
Second Interleave:On
Puncture Limit:0
CCTrCH Length:2100
Number Of Transport Channels:2

Transport Channels:

Item Number 0:

Transport Channel Parameters:

Transport Channel:

Name:D_DCH
Identity:0

TTI (ms):20
EP Type:Turbo Coding
CRC Size:16
RM Attribute:150
First Interleave:On
Number Of Transport Formats:5

Transport Format Set:

Transport Format 0:

Number Of Transport Blocks:0
Transport Block Size In Bits:336

Transport Format 1:

Number Of Transport Blocks:1
Transport Block Size In Bits:336

Transport Format 2:

Number Of Transport Blocks:2
Transport Block Size In Bits:336

Transport Format 3:

Number Of Transport Blocks:3
Transport Block Size In Bits:336

Transport Format 4:

Number Of Transport Blocks:4
Transport Block Size In Bits:336

RM Maximum Length:3928

Item Number 1:

Transport Channel Parameters:

Transport Channel:

Name:D_DCH
Identity:1

TTI (ms):40
EP Type:1/3 Rate Convolutional Coding
CRC Size:16
RM Attribute:170
First Interleave:On
Number Of Transport Formats:2

Transport Format Set:

Transport Format 0:

Number Of Transport Blocks:0
Transport Block Size In Bits:148

Transport Format 1:

Number Of Transport Blocks:1
Transport Block Size In Bits:148

RM Maximum Length:544

Transport Format Combination Set:

Number Of Transport Format Combinations:10

Transport Format Combinations 0:

Transport Format:0
Transport Format:0

Transport Format Combinations 1:

Transport Format:1
Transport Format:0

Transport Format Combinations 2:

Transport Format:2
Transport Format:0

Transport Format Combinations 3:

Transport Format:3
Transport Format:0

Transport Format Combinations 4:

Transport Format:4
Transport Format:0

Transport Format Combinations 5:

Transport Format:0
Transport Format:1

Transport Format Combinations 6:

Transport Format:1
Transport Format:1

Transport Format Combinations 7:

Transport Format:2
Transport Format:1

Transport Format Combinations 8:

Transport Format:3
Transport Format:1

Transport Format Combinations 9:

Transport Format:4
Transport Format:1

#### CPHY Transport Channel Configuration CNF

PHY LLA @ 00:01:03.020

BTS unit: 1:1
Channel No: 0 Name: D_DPCH
CFN: 167

Message Details:

#### CPHY_TrCH_Config_CNF

LLA RRC @ 00:01:03.040

Channel ID: DL-DPCH#1
Cell ID: 0

Message Details:

CPHY_TrCH_Config_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:26

#### CMAC_Config_REQ

RRC LLA @ 00:01:03.040

Channel ID: DL-DPCH#1
Cell ID: -1

Message Details:

CMAC_Config_REQ:

cellId:-1

routingInfo:

physicalChannelIdentity:26

ratType:fdd

configMessage:

reconfigure: (CmacConfigReq)

activationTime: (SS_ActivationTime)

activationCFN (ActivationTime):104

uE_Info:

u_RNTI: Omit

c_RNTI: Omit

trCHInfo:

ulconnectedTrCHList: Omit

ulTFCS: (TFCS) Omit

dlconnectedTrCHList:

:

trchid (TransportChannelIdentity):6

transportChannelInfo: (CommonOrDedicatedTFS)

tti:

tti20: (CommonOrDedicatedTF_InfoList)

CommonOrDedicatedTF_Info:

tb_Size:336

numberOfTbSizeList:

NumberOfTransportBlocks:

zero:

NumberOfTransportBlocks:

one:

NumberOfTransportBlocks:

small:2

NumberOfTransportBlocks:

small:3

NumberOfTransportBlocks:

small:4

logicalChannelList:

allSizes:

semistaticTF_Information:

channelCodingType:

turbo:

rateMatchingAttribute:150
crc_Size:crc16

:

trchid (TransportChannelIdentity):10

transportChannelInfo: (CommonOrDedicatedTFS)

tti:

tti40: (CommonOrDedicatedTF_InfoList)

CommonOrDedicatedTF_Info:

tb_Size:148

numberOfTbSizeList:

NumberOfTransportBlocks:

zero:

NumberOfTransportBlocks:

one:

logicalChannelList:

allSizes:

semistaticTF_Information:

channelCodingType:

convolutional (CodingRate):third

rateMatchingAttribute:170
crc_Size:crc16

dlTFCS: (TFCS)

normalTFCI_Signalling: (ExplicitTFCS_Configuration)

complete: (TFCS_ReconfAdd)

ctfcSize:

ctfc4Bit:

:

ctfc4:0

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:1

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:2

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:3

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:4

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:5

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:6

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:7

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:8

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc4:9

powerOffsetInformation:

gainFactorInformation:

signalledGainFactors:

modeSpecificInfo:

fdd:

gainFactorBetaC (GainFactor):9

gainFactorBetaD (GainFactor):15
referenceTFC_ID:0

powerOffsetPp_m: Omit

trCH_LogCHMapping: (TrCH_LogCHMappingList1)

ulconnectedTrCHList: Omit

dlconnectedTrCHList:

:

trchid (TransportChannelIdentity):6

trCH_LogCHMappingList:

TrCH_LogicalChannelMapping:

logicalChannel_Mapping:

dl_LogicalChannelMapping: (SS_DL_LogicalChannelMapping)

macHeaderManipulation (MAC_HeaderManipulation):normalMacHeader
dl_TransportChannelType (SS_DL_TransportChannelType):dch
logicalChannelIdentity:7
logicalChannelType:dTCH

rlc_SizeList:

configured:

mac_LogicalChannelPriority:8

rB_Identity:20
cn_DomainIdentity: Omit

:

trchid (TransportChannelIdentity):10

trCH_LogCHMappingList:

TrCH_LogicalChannelMapping:

logicalChannel_Mapping:

dl_LogicalChannelMapping: (SS_DL_LogicalChannelMapping)

macHeaderManipulation (MAC_HeaderManipulation):normalMacHeader
dl_TransportChannelType (SS_DL_TransportChannelType):dch
logicalChannelIdentity:1
logicalChannelType:dCCH

rlc_SizeList:

configured:

mac_LogicalChannelPriority:1

rB_Identity:1
cn_DomainIdentity: Omit

TrCH_LogicalChannelMapping:

logicalChannel_Mapping:

dl_LogicalChannelMapping: (SS_DL_LogicalChannelMapping)

macHeaderManipulation (MAC_HeaderManipulation):normalMacHeader
dl_TransportChannelType (SS_DL_TransportChannelType):dch
logicalChannelIdentity:2
logicalChannelType:dCCH

rlc_SizeList:

configured:

mac_LogicalChannelPriority:2

rB_Identity:2
cn_DomainIdentity: Omit

TrCH_LogicalChannelMapping:

logicalChannel_Mapping:

dl_LogicalChannelMapping: (SS_DL_LogicalChannelMapping)

macHeaderManipulation (MAC_HeaderManipulation):normalMacHeader
dl_TransportChannelType (SS_DL_TransportChannelType):dch
logicalChannelIdentity:3
logicalChannelType:dCCH

rlc_SizeList:

configured:

mac_LogicalChannelPriority:3

rB_Identity:3
cn_DomainIdentity: Omit

TrCH_LogicalChannelMapping:

logicalChannel_Mapping:

dl_LogicalChannelMapping: (SS_DL_LogicalChannelMapping)

macHeaderManipulation (MAC_HeaderManipulation):normalMacHeader
dl_TransportChannelType (SS_DL_TransportChannelType):dch
logicalChannelIdentity:4
logicalChannelType:dCCH

rlc_SizeList:

configured:

mac_LogicalChannelPriority:4

rB_Identity:4
cn_DomainIdentity: Omit

#### CMAC Configuration REQ

LLA MAC @ 00:01:03.050

BTS unit: 1:1
Channel No: 0 Name: D_DPCH
CFN: 170

Message Details:

Configuration Parameters:

Activation Time:104
Number Of Transport Channels:2

Transport Channels:

Item Number 0:

Transport Channel Parameters:

Transport Channel:

Name:D_DCH
Identity:0

TTI (ms):20
EP Type:Turbo Coding
CRC Size:16
RM Attribute:150
First Interleave:On
Number Of Transport Formats:5

Transport Format Set:

Transport Format 0:

Number Of Transport Blocks:0
Transport Block Size In Bits:336

Transport Format 1:

Number Of Transport Blocks:1
Transport Block Size In Bits:336

Transport Format 2:

Number Of Transport Blocks:2
Transport Block Size In Bits:336

Transport Format 3:

Number Of Transport Blocks:3
Transport Block Size In Bits:336

Transport Format 4:

Number Of Transport Blocks:4
Transport Block Size In Bits:336

Number Of Logical Channels:1

Logical Channels:

Item Number 0:

Logical Channel:

Name:D_DTCH
Identity:4

Priority:8
CT Length:0
CT Value:0
TCTF Length:0
TCTF Value:0
UE ID Type:Not used
UE ID:0

Item Number 1:

Transport Channel Parameters:

Transport Channel:

Name:D_DCH
Identity:1

TTI (ms):40
EP Type:1/3 Rate Convolutional Coding
CRC Size:16
RM Attribute:170
First Interleave:On
Number Of Transport Formats:2

Transport Format Set:

Transport Format 0:

Number Of Transport Blocks:0
Transport Block Size In Bits:148

Transport Format 1:

Number Of Transport Blocks:1
Transport Block Size In Bits:148

Number Of Logical Channels:4

Logical Channels:

Item Number 0:

Logical Channel:

Name:DCCH
Identity:1

Priority:1
CT Length:4
CT Value:0
TCTF Length:0
TCTF Value:0
UE ID Type:Not used
UE ID:0

Item Number 1:

Logical Channel:

Name:DCCH
Identity:2

Priority:2
CT Length:4
CT Value:1
TCTF Length:0
TCTF Value:0
UE ID Type:Not used
UE ID:0

Item Number 2:

Logical Channel:

Name:DCCH
Identity:3

Priority:3
CT Length:4
CT Value:2
TCTF Length:0
TCTF Value:0
UE ID Type:Not used
UE ID:0

Item Number 3:

Logical Channel:

Name:DCCH
Identity:4

Priority:4
CT Length:4
CT Value:3
TCTF Length:0
TCTF Value:0
UE ID Type:Not used
UE ID:0

Active Flag:1

Transport Format Combination Set:

Number Of Transport Format Combinations:10

Transport Format Combinations 0:

Transport Format:0
Transport Format:0

Transport Format Combinations 1:

Transport Format:1
Transport Format:0

Transport Format Combinations 2:

Transport Format:2
Transport Format:0

Transport Format Combinations 3:

Transport Format:3
Transport Format:0

Transport Format Combinations 4:

Transport Format:4
Transport Format:0

Transport Format Combinations 5:

Transport Format:0
Transport Format:1

Transport Format Combinations 6:

Transport Format:1
Transport Format:1

Transport Format Combinations 7:

Transport Format:2
Transport Format:1

Transport Format Combinations 8:

Transport Format:3
Transport Format:1

Transport Format Combinations 9:

Transport Format:4
Transport Format:1

#### CMAC Configuration CNF

MAC LLA @ 00:01:03.060

BTS unit: 1:1
Channel No: 0 Name: D_DPCH
CFN: 171

Message Details:

#### PHY_DATA_IND

PHY MAC @ 00:01:03.110

BTS unit: 1:1
Channel No: 0 Name: U_DCH
CFN: 156

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]10 20 07 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]02 00 70 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### MAC_DATA_IND

MAC RLC @ 00:01:03.110

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 156

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 70 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:7

#### CMAC_Config_CNF

LLA RRC @ 00:01:03.770

Channel ID: DL-DPCH#1
Cell ID: -1

Message Details:

CMAC_Config_CNF:

cellId:-1

routingInfo:

physicalChannelIdentity:26

#### CPHY_RL_Modify_REQ

RRC LLA @ 00:01:03.770

Channel ID: UL-DPCH#1
Cell ID: 0

Message Details:

CPHY_RL_Modify_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:20

ratType:fdd

modifyMessage: (CphyRlModifyReq)

activationTime: (SS_ActivationTime)

activationCFN (ActivationTime):104

physicalChannelInfo:

dPCHInfo:

ul_DPCHInfo: (UL_DPCH_Info)

ul_DPCH_PowerControlInfo:

fdd:

dpcch_PowerOffset:-40
pc_Preamble:1
sRB_delay:7

powerControlAlgorithm:

algorithm1 (TPC_StepSizeFDD):1

modeSpecificInfo:

fdd:

scramblingCodeType:longSC
scramblingCode (UL_ScramblingCode):0
numberOfDPDCH: Omit
spreadingFactor:sf16
tfci_Existence:true
numberOfFBI_Bits: Omit
puncturingLimit:pl0_96

dl_DPCHInfo: Omit

#### CPHY Radio Link Setup REQ

LLA PHY @ 00:01:03.910

BTS unit: 1:1
Channel No: 0 Name: U_DPCH
CFN: 0

Message Details:

Configuration Parameters:

Activation Time:104
Channel Offset:8704
Scrambling Code:16777216
Symbol Rate:240k
Channelization Code:0
Adjust Time:0
Slot Format:0
Number Of DPDCH:1

DPDCH Parameters:

Item Number 0:

Channelization Code:4

#### CPHY Radio Link Setup CNF

PHY LLA @ 00:01:03.910

BTS unit: 1:1
Channel No: 0 Name: U_DPCH
CFN: 0

Message Details:

#### CPHY Transport Channel Configuration REQ

LLA PHY @ 00:01:03.960

BTS unit: 1:1
Channel No: 0 Name: U_DPCH
CFN: 5

Message Details:

Configuration Parameters:

Activation Time:104
DTX Position:Flexible
Second Interleave:On
Puncture Limit:96
CCTrCH Length:1200
Number Of Transport Channels:1

Transport Channels:

Item Number 0:

Transport Channel Parameters:

Transport Channel:

Name:U_DCH
Identity:0

TTI (ms):10
EP Type:1/3 Rate Convolutional Coding
CRC Size:16
RM Attribute:192
First Interleave:On
Number Of Transport Formats:2

Transport Format Set:

Transport Format 0:

Number Of Transport Blocks:0
Transport Block Size In Bits:148

Transport Format 1:

Number Of Transport Blocks:1
Transport Block Size In Bits:148

RM Maximum Length:960

Transport Format Combination Set:

Number Of Transport Format Combinations:2

Transport Format Combinations 0:

Transport Format:0

Transport Format Combinations 1:

Transport Format:1

#### CPHY Transport Channel Configuration CNF

PHY LLA @ 00:01:03.980

BTS unit: 1:1
Channel No: 0 Name: U_DPCH
CFN: 7

Message Details:

#### CPHY_RL_Modify_CNF

LLA RRC @ 00:01:04.010

Channel ID: UL-DPCH#1
Cell ID: 0

Message Details:

CPHY_RL_Modify_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:20

#### CPHY_TrCH_Config_REQ

RRC LLA @ 00:01:04.010

Channel ID: UL-DPCH#1
Cell ID: 0

Message Details:

CPHY_TrCH_Config_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:20

ratType:fdd

trchConfigType:

dch:Normal

configMessage: (CphyTrchConfigReq)

activationTime: (SS_ActivationTime)

activationCFN (ActivationTime):104

ulconnectedTrCHList:

:

trchid (TransportChannelIdentity):1
ul_TransportChannelType (SS_UL_TransportChannelType):dch

transportChannelInfo: (CommonOrDedicatedTFS)

tti:

tti20: (CommonOrDedicatedTF_InfoList)

CommonOrDedicatedTF_Info:

tb_Size:336

numberOfTbSizeList:

NumberOfTransportBlocks:

zero:

NumberOfTransportBlocks:

one:

NumberOfTransportBlocks:

small:2

NumberOfTransportBlocks:

small:3

NumberOfTransportBlocks:

small:4

logicalChannelList:

allSizes:

semistaticTF_Information:

channelCodingType:

turbo:

rateMatchingAttribute:150
crc_Size:crc16

:

trchid (TransportChannelIdentity):5
ul_TransportChannelType (SS_UL_TransportChannelType):dch

transportChannelInfo: (CommonOrDedicatedTFS)

tti:

tti40: (CommonOrDedicatedTF_InfoList)

CommonOrDedicatedTF_Info:

tb_Size:148

numberOfTbSizeList:

NumberOfTransportBlocks:

zero:

NumberOfTransportBlocks:

one:

logicalChannelList:

allSizes:

semistaticTF_Information:

channelCodingType:

convolutional (CodingRate):third

rateMatchingAttribute:170
crc_Size:crc16

ulTFCS: (TFCS)

normalTFCI_Signalling: (ExplicitTFCS_Configuration)

complete: (TFCS_ReconfAdd)

ctfcSize:

ctfc4Bit:

:

ctfc4:0

powerOffsetInformation: Omit

:

ctfc4:1

powerOffsetInformation: Omit

:

ctfc4:2

powerOffsetInformation: Omit

:

ctfc4:3

powerOffsetInformation: Omit

:

ctfc4:4

powerOffsetInformation: Omit

:

ctfc4:5

powerOffsetInformation: Omit

:

ctfc4:6

powerOffsetInformation: Omit

:

ctfc4:7

powerOffsetInformation: Omit

:

ctfc4:8

powerOffsetInformation: Omit

:

ctfc4:9

powerOffsetInformation: Omit

dlconnectedTrCHList: Omit

dlTFCS: (TFCS) Omit

#### CPHY Radio Link Setup REQ

LLA PHY @ 00:01:04.070

BTS unit: 1:1
Channel No: 0 Name: U_DPCH
CFN: 16

Message Details:

Configuration Parameters:

Activation Time:104
Channel Offset:8704
Scrambling Code:16777216
Symbol Rate:240k
Channelization Code:0
Adjust Time:0
Slot Format:0
Number Of DPDCH:1

DPDCH Parameters:

Item Number 0:

Channelization Code:4

#### CPHY Radio Link Setup CNF

PHY LLA @ 00:01:04.070

BTS unit: 1:1
Channel No: 0 Name: U_DPCH
CFN: 16

Message Details:

#### CPHY Transport Channel Configuration REQ

LLA PHY @ 00:01:04.100

BTS unit: 1:1
Channel No: 0 Name: U_DPCH
CFN: 19

Message Details:

Configuration Parameters:

Activation Time:104
DTX Position:Flexible
Second Interleave:On
Puncture Limit:96
CCTrCH Length:2400
Number Of Transport Channels:2

Transport Channels:

Item Number 0:

Transport Channel Parameters:

Transport Channel:

Name:U_DCH
Identity:0

TTI (ms):20
EP Type:Turbo Coding
CRC Size:16
RM Attribute:150
First Interleave:On
Number Of Transport Formats:5

Transport Format Set:

Transport Format 0:

Number Of Transport Blocks:0
Transport Block Size In Bits:336

Transport Format 1:

Number Of Transport Blocks:1
Transport Block Size In Bits:336

Transport Format 2:

Number Of Transport Blocks:2
Transport Block Size In Bits:336

Transport Format 3:

Number Of Transport Blocks:3
Transport Block Size In Bits:336

Transport Format 4:

Number Of Transport Blocks:4
Transport Block Size In Bits:336

RM Maximum Length:2400

Item Number 1:

Transport Channel Parameters:

Transport Channel:

Name:U_DCH
Identity:1

TTI (ms):40
EP Type:1/3 Rate Convolutional Coding
CRC Size:16
RM Attribute:170
First Interleave:On
Number Of Transport Formats:2

Transport Format Set:

Transport Format 0:

Number Of Transport Blocks:0
Transport Block Size In Bits:148

Transport Format 1:

Number Of Transport Blocks:1
Transport Block Size In Bits:148

RM Maximum Length:291

Transport Format Combination Set:

Number Of Transport Format Combinations:10

Transport Format Combinations 0:

Transport Format:0
Transport Format:0

Transport Format Combinations 1:

Transport Format:1
Transport Format:0

Transport Format Combinations 2:

Transport Format:2
Transport Format:0

Transport Format Combinations 3:

Transport Format:3
Transport Format:0

Transport Format Combinations 4:

Transport Format:4
Transport Format:0

Transport Format Combinations 5:

Transport Format:0
Transport Format:1

Transport Format Combinations 6:

Transport Format:1
Transport Format:1

Transport Format Combinations 7:

Transport Format:2
Transport Format:1

Transport Format Combinations 8:

Transport Format:3
Transport Format:1

Transport Format Combinations 9:

Transport Format:4
Transport Format:1

#### CPHY Transport Channel Configuration CNF

PHY LLA @ 00:01:04.120

BTS unit: 1:1
Channel No: 0 Name: U_DPCH
CFN: 21

Message Details:

#### CPHY_TrCH_Config_CNF

LLA RRC @ 00:01:04.150

Channel ID: UL-DPCH#1
Cell ID: 0

Message Details:

CPHY_TrCH_Config_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:20

#### CMAC_Config_REQ

RRC LLA @ 00:01:04.150

Channel ID: UL-DPCH#1
Cell ID: -1

Message Details:

CMAC_Config_REQ:

cellId:-1

routingInfo:

physicalChannelIdentity:20

ratType:fdd

configMessage:

reconfigure: (CmacConfigReq)

activationTime: (SS_ActivationTime)

activationCFN (ActivationTime):104

uE_Info:

u_RNTI: Omit

c_RNTI: Omit

trCHInfo:

ulconnectedTrCHList:

:

trchid (TransportChannelIdentity):1

transportChannelInfo: (CommonOrDedicatedTFS)

tti:

tti20: (CommonOrDedicatedTF_InfoList)

CommonOrDedicatedTF_Info:

tb_Size:336

numberOfTbSizeList:

NumberOfTransportBlocks:

zero:

NumberOfTransportBlocks:

one:

NumberOfTransportBlocks:

small:2

NumberOfTransportBlocks:

small:3

NumberOfTransportBlocks:

small:4

logicalChannelList:

allSizes:

semistaticTF_Information:

channelCodingType:

turbo:

rateMatchingAttribute:150
crc_Size:crc16

:

trchid (TransportChannelIdentity):5

transportChannelInfo: (CommonOrDedicatedTFS)

tti:

tti40: (CommonOrDedicatedTF_InfoList)

CommonOrDedicatedTF_Info:

tb_Size:148

numberOfTbSizeList:

NumberOfTransportBlocks:

zero:

NumberOfTransportBlocks:

one:

logicalChannelList:

allSizes:

semistaticTF_Information:

channelCodingType:

convolutional (CodingRate):third

rateMatchingAttribute:170
crc_Size:crc16

ulTFCS: (TFCS)

normalTFCI_Signalling: (ExplicitTFCS_Configuration)

complete: (TFCS_ReconfAdd)

ctfcSize:

ctfc4Bit:

:

ctfc4:0

powerOffsetInformation: Omit

:

ctfc4:1

powerOffsetInformation: Omit

:

ctfc4:2

powerOffsetInformation: Omit

:

ctfc4:3

powerOffsetInformation: Omit

:

ctfc4:4

powerOffsetInformation: Omit

:

ctfc4:5

powerOffsetInformation: Omit

:

ctfc4:6

powerOffsetInformation: Omit

:

ctfc4:7

powerOffsetInformation: Omit

:

ctfc4:8

powerOffsetInformation: Omit

:

ctfc4:9

powerOffsetInformation: Omit

dlconnectedTrCHList: Omit

dlTFCS: (TFCS) Omit

trCH_LogCHMapping: (TrCH_LogCHMappingList1)

ulconnectedTrCHList:

:

trchid (TransportChannelIdentity):1

trCH_LogCHMappingList:

TrCH_LogicalChannelMapping:

logicalChannel_Mapping:

ul_LogicalChannelMapping: (SS_UL_LogicalChannelMapping)

macHeaderManipulation (MAC_HeaderManipulation):normalMacHeader
ul_TransportChannelType (SS_UL_TransportChannelType):dch
logicalChannelIdentity:7
logicalChannelType:dTCH

rB_Identity:20
cn_DomainIdentity: Omit

:

trchid (TransportChannelIdentity):5

trCH_LogCHMappingList:

TrCH_LogicalChannelMapping:

logicalChannel_Mapping:

ul_LogicalChannelMapping: (SS_UL_LogicalChannelMapping)

macHeaderManipulation (MAC_HeaderManipulation):normalMacHeader
ul_TransportChannelType (SS_UL_TransportChannelType):dch
logicalChannelIdentity:1
logicalChannelType:dCCH

rB_Identity:1
cn_DomainIdentity: Omit

TrCH_LogicalChannelMapping:

logicalChannel_Mapping:

ul_LogicalChannelMapping: (SS_UL_LogicalChannelMapping)

macHeaderManipulation (MAC_HeaderManipulation):normalMacHeader
ul_TransportChannelType (SS_UL_TransportChannelType):dch
logicalChannelIdentity:2
logicalChannelType:dCCH

rB_Identity:2
cn_DomainIdentity: Omit

TrCH_LogicalChannelMapping:

logicalChannel_Mapping:

ul_LogicalChannelMapping: (SS_UL_LogicalChannelMapping)

macHeaderManipulation (MAC_HeaderManipulation):normalMacHeader
ul_TransportChannelType (SS_UL_TransportChannelType):dch
logicalChannelIdentity:3
logicalChannelType:dCCH

rB_Identity:3
cn_DomainIdentity: Omit

TrCH_LogicalChannelMapping:

logicalChannel_Mapping:

ul_LogicalChannelMapping: (SS_UL_LogicalChannelMapping)

macHeaderManipulation (MAC_HeaderManipulation):normalMacHeader
ul_TransportChannelType (SS_UL_TransportChannelType):dch
logicalChannelIdentity:4
logicalChannelType:dCCH

rB_Identity:4
cn_DomainIdentity: Omit

dlconnectedTrCHList: Omit

#### CMAC Configuration REQ

LLA MAC @ 00:01:04.170

BTS unit: 1:1
Channel No: 0 Name: U_DPCH
CFN: 26

Message Details:

Configuration Parameters:

Activation Time:104
Number Of Transport Channels:2

Transport Channels:

Item Number 0:

Transport Channel Parameters:

Transport Channel:

Name:U_DCH
Identity:0

TTI (ms):20
EP Type:Turbo Coding
CRC Size:16
RM Attribute:150
First Interleave:On
Number Of Transport Formats:5

Transport Format Set:

Transport Format 0:

Number Of Transport Blocks:0
Transport Block Size In Bits:336

Transport Format 1:

Number Of Transport Blocks:1
Transport Block Size In Bits:336

Transport Format 2:

Number Of Transport Blocks:2
Transport Block Size In Bits:336

Transport Format 3:

Number Of Transport Blocks:3
Transport Block Size In Bits:336

Transport Format 4:

Number Of Transport Blocks:4
Transport Block Size In Bits:336

Number Of Logical Channels:1

Logical Channels:

Item Number 0:

Logical Channel:

Name:U_DTCH
Identity:4

Priority:0
CT Length:0
CT Value:0
TCTF Length:0
TCTF Value:0
UE ID Type:Not used
UE ID:0

Item Number 1:

Transport Channel Parameters:

Transport Channel:

Name:U_DCH
Identity:1

TTI (ms):40
EP Type:1/3 Rate Convolutional Coding
CRC Size:16
RM Attribute:170
First Interleave:On
Number Of Transport Formats:2

Transport Format Set:

Transport Format 0:

Number Of Transport Blocks:0
Transport Block Size In Bits:148

Transport Format 1:

Number Of Transport Blocks:1
Transport Block Size In Bits:148

Number Of Logical Channels:4

Logical Channels:

Item Number 0:

Logical Channel:

Name:DCCH
Identity:1

Priority:0
CT Length:4
CT Value:0
TCTF Length:0
TCTF Value:0
UE ID Type:Not used
UE ID:0

Item Number 1:

Logical Channel:

Name:DCCH
Identity:2

Priority:0
CT Length:4
CT Value:1
TCTF Length:0
TCTF Value:0
UE ID Type:Not used
UE ID:0

Item Number 2:

Logical Channel:

Name:DCCH
Identity:3

Priority:0
CT Length:4
CT Value:2
TCTF Length:0
TCTF Value:0
UE ID Type:Not used
UE ID:0

Item Number 3:

Logical Channel:

Name:DCCH
Identity:4

Priority:0
CT Length:4
CT Value:3
TCTF Length:0
TCTF Value:0
UE ID Type:Not used
UE ID:0

Active Flag:1

Transport Format Combination Set:

Number Of Transport Format Combinations:10

Transport Format Combinations 0:

Transport Format:0
Transport Format:0

Transport Format Combinations 1:

Transport Format:1
Transport Format:0

Transport Format Combinations 2:

Transport Format:2
Transport Format:0

Transport Format Combinations 3:

Transport Format:3
Transport Format:0

Transport Format Combinations 4:

Transport Format:4
Transport Format:0

Transport Format Combinations 5:

Transport Format:0
Transport Format:1

Transport Format Combinations 6:

Transport Format:1
Transport Format:1

Transport Format Combinations 7:

Transport Format:2
Transport Format:1

Transport Format Combinations 8:

Transport Format:3
Transport Format:1

Transport Format Combinations 9:

Transport Format:4
Transport Format:1

#### CMAC Configuration CNF

MAC LLA @ 00:01:04.170

BTS unit: 1:1
Channel No: 0 Name: U_DPCH
CFN: 26

Message Details:

#### CMAC_Config_CNF

LLA RRC @ 00:01:04.190

Channel ID: UL-DPCH#1
Cell ID: -1

Message Details:

CMAC_Config_CNF:

cellId:-1

routingInfo:

physicalChannelIdentity:20

#### CRLC_Config_REQ

RRC LLA @ 00:01:04.190

Channel ID: Rb20
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:20

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode)

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw128

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):320

dl_RLCModeInfo: (UL_RLC_Mode)

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw128
timerRST:tr500
max_RST (MaxRST):rst4

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity):7
dLlogicalChannelIdentity (LogicalChannelIdentity):7
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC AM Channel Establish REQ

LLA RLC @ 00:01:04.230

BTS unit: 1:1
Channel No: 4 Name: D_DTCH
CFN: 32

Message Details:

Configuration Parameters:

PU Size In Bits:320

Timer Parameters:

Poll (ms):200
Poll Prohibit (ms):0
EPC (ms):0
Discard (ms):0
Poll Periodic (ms):0
Status Prohibit (ms):0
Status Periodic (ms):0
Reset (ms):500
MRW (ms):0

Protocol Parameters:

Max Dat:15
Poll PU:0
Poll SDU:1
Poll Window:99
Max Reset:4
Tx Window Size:128
Rx Window Size:128
Max MRW:0
SDU Discard Mode:No discard

Polling Triggers:

Last PU In Buffer:On
Last PU In Retransmission Buffer:On
Poll Timer:On
Every Poll-PU PU:Off
Every Poll-SDU SDU:On
Poll-Window Percent Of Transmission Buffer:On
Timer Based:Off

Status Triggers:

Missing PU:On
Timer Based:Off
EPC Mechanism:Off

#### CRLC AM Channel Establish CNF

RLC LLA @ 00:01:04.230

BTS unit: 1:1
Channel No: 4 Name: D_DTCH
CFN: 32

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:01:04.240

Channel ID: Rb20
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:20

#### PHY_DATA_IND

PHY MAC @ 00:01:05.190

BTS unit: 1:1
Channel No: 1 Name: U_DCH
CFN: 108

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 01 D1 3F ED 55 79 DA
[8]C9 3C 80 00 00 45 55 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 1D 13 FE D5 57 9D AC
[8]93 C8 00 00 04 55 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:01:05.190

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 108

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 1D 13 FE D5 57 9D AC
[8]93 C8 00 00 04 55 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:3
Polling bit:1 (request a status report)
Length indicator 0 (octets):9
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (9 octets):

[0]D5 57 9D AC 93 C8 00 00
[8]04
Padding associated with length indicator 1 (5 octets):

[0]55 55 55 55 55

#### MAC_DATA_REQ

RLC MAC @ 00:01:05.200

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 129

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 40 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:4

#### CMAC Integrity Check Request

RRC MAC @ 00:01:05.220

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000010
Data:

[0]00 00 00 02
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:0 (UE to RNC)
Message Length (bits):72
Message:

[0]80 00 00 01 03 C8 00 00
[8]04

#### RLC_AM_DATA_IND: radioBearerSetupComplete

RLC LLA @ 00:01:05.220

Channel No: 2 Name: DCCH

Message Details:

UL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode: 10101010101011110011101101011001

rrc_MessageSequenceNumber: 2

message:

radioBearerSetupComplete:

rrc_TransactionIdentifier: 0

ul_IntegProtActivationInfo: Omitted

ul_TimingAdvance: Omitted

start_Value: 00000000000000000010

count_C_ActivationTime: Omitted

rb_UL_CiphActivationTimeInfo: Omitted

ul_CounterSynchronisationInfo: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]D5 57 9D AC 93 C8 00 00
[8]04

#### CMAC Integrity Check Result

MAC RRC @ 00:01:05.220

Message Details:

Integrity Check Result:

MAC-I:10101010101011110011101101011001
Data:

[0]AA AF 3B 59

#### RLC_AM_DATA_IND

LLA RRC @ 00:01:05.220

Channel ID: Rb2
Cell ID: -1

Message Details:

RLC_AM_DATA_IND:

cellId:-1

routingInfo:

rB_Identity:2

integrityResult:

integrityUsed (IntegrityStatus):i_pass

aM_message:

uL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode:10101010101011110011101101011001
rrc_MessageSequenceNumber:2

message: (UL_DCCH_MessageType)

radioBearerSetupComplete:

rrc_TransactionIdentifier:0

ul_IntegProtActivationInfo: (IntegrityProtActivationInfo) Omit

ul_TimingAdvance: Omit
start_Value:00000000000000000010
count_C_ActivationTime (ActivationTime): Omit

rb_UL_CiphActivationTimeInfo: (RB_ActivationTimeInfoList) Omit

ul_CounterSynchronisationInfo: Omit

laterNonCriticalExtensions: Omit

#### CRLC_SecurityMode_Config_REQ

RRC LLA @ 00:01:05.220

Cell ID: -1

Message Details:

CRLC_SecurityMode_Config_REQ:

cellId:-1

rlcSecurityInfo: (SecurityInfo)

cn_DomainIdentity:ps_domain
startValue (START_Value):00000000000000000010
cipheringKey: Omit
integrityKey: Omit
gsmCipheringKey: Omit

#### CRLC_SecurityMode_Config_REQ

RRC RLC @ 00:01:05.220

Message Details:

cellIdentity: 1

rlcSecurityInfo:

cn_DomainIdentity: ps_domain_CN_DomainIdentity

startValue: 00000000000000000010

cipheringKey: Omitted

integrityKey: Omitted

#### PHY_DATA_REQ

MAC PHY @ 00:01:05.230

BTS unit: 1:1
Channel No: 1 Name: DCH
CFN: 132

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]10 20 04 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]02 00 40 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### CMAC Integrity Check Request

RRC MAC @ 00:01:05.240

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000001
Data:

[0]00 00 00 01
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:1 (RNC to UE)
Message Length (bits):216
Message:

[0]80 00 00 01 81 42 02 51
[8]48 40 01 63 68 63 ED 44
[16]08 08 0E 9F E2 02 00 26
[24]80 20 00

#### CMAC Integrity Check Result

MAC RRC @ 00:01:05.240

Message Details:

Integrity Check Result:

MAC-I:01101001110101110111011100011101
Data:

[0]69 D7 77 1D

#### CRLC_SecurityMode_Config_CNF

LLA RRC @ 00:01:05.240

Cell ID: -1

Message Details:

CRLC_SecurityMode_Config_CNF:

cellId:-1

#### RRC_DATA_REQ: sm:activatePdpContextAccept

NAS RRC @ 00:01:05.240

Cell ID: -1

Message Details:

ACTIVATEPDPCONTEXTACCEPTdl:

ti:

tiFlag: 1

tiVal: 000

sM_ProtocolDiscriminator: 1010

msgType: 01000010

negiotiatedLLC_SAPI:

spare: 0000

nSAPI_Value: 0000

negiotiatedQoS:

length: 0B

spare: 00

dlyClass: 011

relabilityClass: 011

peakThroughput: 0100

spare1: 0

precedenceClass: 011

spare2: 000

meanThroughput: 11111

trafficClass: 011

deliveryOrder: 01

deliveryErrorSDU: 010

maxSDUSize: 20

maxBitRateUplink: 40

maxBitRateDnlink: 40

residualBER: 0111

sduErrRatio: 0100

transDly: 111111

trafficHandpro: 11

bitRateUplink: 10

bitRateDnlink: 10

spare: 0000

radioPriority:

spare: 0

value: 001

pDP_Address: Omitted

protocolConfOpts: Omitted

pktFlowID:

iei: 00110100

length: 01

pktFlowIdentifier: 00

#### RLC_AM_DATA_REQ:downlinkDirectTransfer

RRC RLC @ 00:01:05.240

Channel No: 3 Name: DCCH

Message Details:

Opt1: 0

Opt2: 0

DL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode: 01101001110101110111011100011101

rrc_MessageSequenceNumber: 1

message:

downlinkDirectTransfer:

r3:

downlinkDirectTransfer_r3:

rrc_TransactionIdentifier: 0

cn_DomainIdentity: ps_domain_CN_DomainIdentity [enum=1]

nas_Message: 8A42000B1B431F6A20404074FF101001340100

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]B4 EB BB 8E 89 42 02 51
[8]48 40 01 63 68 63 ED 44
[16]08 08 0E 9F E2 02 00 26
[24]80 20 00

#### RLC_AM_DATA_REQ

RRC LLA @ 00:01:05.240

Channel ID: Rb2
Cell ID: -1

Message Details:

RLC_AM_DATA_REQ:

cellId:-1

routingInfo:

rB_Identity:2

confirmationRequest: (AmConfirmationRequest)

noConfirmationRequest:

aM_message:

dL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode:00000000000000000000000000000000
rrc_MessageSequenceNumber:0

message: (DL_DCCH_MessageType)

measurementControl:

r3:

measurementControl_r3: (MeasurementControl_r3_IEs)

rrc_TransactionIdentifier:0
measurementIdentity:4

measurementCommand:

setup: (MeasurementType)

interFrequencyMeasurement:

interFreqCellInfoList:

removedInterFreqCellList: Omit

newInterFreqCellList:

NewInterFreqCell:

interFreqCellID:3

frequencyInfo:

modeSpecificInfo:

fdd: (FrequencyInfoFDD)

uarfcn_UL (UARFCN): Omit
uarfcn_DL (UARFCN):10837

cellInfo:

cellIndividualOffset: Omit

referenceTimeDifferenceToCell: Omit

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode:250

primaryCPICH_TX_Power: Omit
readSFN_Indicator:false
tx_DiversityIndicator:false

cellsForInterFreqMeasList: Omit

interFreqMeasQuantity:

reportingCriteria:

interFreqReportingCriteria:

filterCoefficient:fc4

modeSpecificInfo:

fdd:

freqQualityEstimateQuantity_FDD:cpich_RSCP

interFreqReportingQuantity:

utra_Carrier_RSSI:false
frequencyQualityEstimate:false

nonFreqRelatedQuantities: (CellReportingQuantities)

dummy (SFN_SFN_OTD_Type):noReport
cellIdentity_reportingIndicator:false
cellSynchronisationInfoReportingIndicator:false

modeSpecificInfo:

fdd:

cpich_Ec_N0_reportingIndicator:false
cpich_RSCP_reportingIndicator:true
pathloss_reportingIndicator:false

measurementValidity: Omit

interFreqSetUpdate: (UE_AutonomousUpdateMode)

onWithNoReporting:

reportCriteria: (InterFreqReportCriteria)

interFreqReportingCriteria:

interFreqEventList:

InterFreqEvent:

event2e:

hysteresis (HysteresisInterFreq):1
timeToTrigger:ttt5000

reportingCellStatus: Omit

nonUsedFreqParameterList:

NonUsedFreqParameter:

nonUsedFreqThreshold (Threshold):-70
nonUsedFreqW (W):0

InterFreqEvent:

event2b:

usedFreqThreshold (Threshold):-70
usedFreqW (W):4
hysteresis (HysteresisInterFreq):1
timeToTrigger:ttt5000

reportingCellStatus:

withinActSetOrVirtualActSet_InterRATcells (MaxNumberOfReportingCellsType2):e1

nonUsedFreqParameterList:

NonUsedFreqParameter:

nonUsedFreqThreshold (Threshold):-70
nonUsedFreqW (W):0

measurementReportingMode:

measurementReportTransferMode (TransferMode):unacknowledgedModeRLC
periodicalOrEventTrigger:eventTrigger

additionalMeasurementList: (AdditionalMeasurementID_List) Omit

dpch_CompressedModeStatusInfo: Omit

v390nonCriticalExtensions: Omit

#### CMAC Integrity Check Request

RRC MAC @ 00:01:05.260

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000011
Data:

[0]00 00 00 03
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:1 (RNC to UE)
Message Length (bits):216
Message:

[0]80 00 00 01 02 08 18 75
[8]03 19 52 A8 9F 46 88 04
[16]B3 10 F8 5A 03 AD 20 7F
[24]00 2D 06

#### RLC_AM_DATA_REQ: measurementControl

LLA RLC @ 00:01:05.260

Channel No: 2 Name: DCCH

Message Details:

DL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode: 10110100100100010011100110111110

rrc_MessageSequenceNumber: 3

message:

measurementControl:

r3:

measurementControl_r3:

rrc_TransactionIdentifier: 0

measurementIdentity: 4

measurementCommand:

setup:

interFrequencyMeasurement:

interFreqCellInfoList:

removedInterFreqCellList: Omitted

newInterFreqCellList:

NewInterFreqCellList.element:

interFreqCellID: 3

frequencyInfo:

modeSpecificInfo:

fdd:

uarfcn_UL: Omitted

uarfcn_DL: 10837

cellInfo:

cellIndividualOffset: Default

referenceTimeDifferenceToCell: Omitted

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode: 250

primaryCPICH_TX_Power: Omitted

readSFN_Indicator: 0

tx_DiversityIndicator: 0

cellsForInterFreqMeasList: Omitted

interFreqMeasQuantity:

reportingCriteria:

interFreqReportingCriteria:

filterCoefficient: fc4_FilterCoefficient [enum=4]

modeSpecificInfo:

fdd:

freqQualityEstimateQuantity_FDD: cpich_RSCP_FreqQualityEstimateQuantity_FDD [enum=1]

interFreqReportingQuantity:

utra_Carrier_RSSI: 0

frequencyQualityEstimate: 0

nonFreqRelatedQuantities:

dummy: noReport_SFN_SFN_OTD_Type [enum=0]

cellIdentity_reportingIndicator: 0

cellSynchronisationInfoReportingIndicator: 0

modeSpecificInfo:

fdd:

cpich_Ec_N0_reportingIndicator: 0

cpich_RSCP_reportingIndicator: 1

pathloss_reportingIndicator: 0

measurementValidity: Omitted

interFreqSetUpdate:

onWithNoReporting: NULL

reportCriteria:

interFreqReportingCriteria:

interFreqEventList:

InterFreqEventList.element:

event2e:

hysteresis: 1

timeToTrigger: ttt5000_TimeToTrigger [enum=15]

reportingCellStatus: Omitted

nonUsedFreqParameterList:

NonUsedFreqParameterList.element:

nonUsedFreqThreshold: -70

nonUsedFreqW: 0

InterFreqEventList.element:

event2b:

usedFreqThreshold: -70

usedFreqW: 4

hysteresis: 1

timeToTrigger: ttt5000_TimeToTrigger [enum=15]

reportingCellStatus:

withinActSetOrVirtualActSet_InterRATcells: e1_MaxNumberOfReportingCellsType2 [enum=0]

nonUsedFreqParameterList:

NonUsedFreqParameterList.element:

nonUsedFreqThreshold: -70

nonUsedFreqW: 0

measurementReportingMode:

measurementReportTransferMode: unacknowledgedModeRLC_TransferMode [enum=1]

periodicalOrEventTrigger: eventTrigger_PeriodicalOrEventTrigger [enum=1]

additionalMeasurementList: Omitted

dpch_CompressedModeStatusInfo: Omitted

v390nonCriticalExtensions: Omitted

Layer 3 SDU:

[0]DA 48 9C DF 1A 08 18 75
[8]03 19 52 A8 9F 46 88 04
[16]B3 10 F8 5A 03 AD 20 7F
[24]00 2D 06

#### CMAC Integrity Check Result

MAC RRC @ 00:01:05.260

Message Details:

Integrity Check Result:

MAC-I:10110100100100010011100110111110
Data:

[0]B4 91 39 BE

#### CPHY_Frame_Number_REQ

RRC LLA @ 00:01:05.260

Channel ID: DL-DPCH#1
Cell ID: 0

Message Details:

CPHY_Frame_Number_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:26

#### CPHY BTS Monitor & SFN CNF

PHY RRC @ 00:01:05.350

BTS unit: 1:1
CFN: 144

Message Details:

SFN:144
Tx Attenuation in dB:5
Rx Ref Power in dBm:0
TxP_SCH in dBm:-45
TxS_SCH in dBm:-45
TxP_CPICH in dBm:-40
TxP_CCPCH in dBm:-42
TxS_CCPCH in dBm:-42
TxDPSCH in dBm:-
TxPICH in dBm:-45
TxAICH in dBm:-45
TxDPCCH in dBm:-45
TxDPDCH1 in dBm:-45
TxDPDCH2 in dBm:-
TxDPDCH3 in dBm:-
TxAWGN in dBm:-
RxTotal in dBm:21.3
RxPRACH in dBm:-17.7
RxPCPCH in dBm:-
RxDPCCH in dBm:20.3
RxDPDCH1 in dBm:-22.1
RxDPDCH2 in dBm:-
RxDPDCH3 in dBm:-
FreqError in Hz:-2
TimingError in chip:0.4

#### MAC_DATA_REQ

RLC MAC @ 00:01:05.350

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 144

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 18 B4 EB BB 8E 89 42
[8]02 51 48 40 01 63 68 63
[16]ED 44

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:3
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]B4 EB BB 8E 89 42 02 51
[8]48 40 01 63 68 63 ED 44

#### MAC_DATA_REQ

RLC MAC @ 00:01:05.350

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 144

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 25 17 FE 08 08 0E 9F
[8]E2 02 00 26 80 20 00 00
[16]00 00

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:4
Polling bit:1 (request a status report)
Length indicator 0 (octets):11
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (11 octets):

[0]08 08 0E 9F E2 02 00 26
[8]80 20 00
Padding associated with length indicator 1 (3 octets):

[0]00 00 00

#### CMAC Integrity Check Request

RRC MAC @ 00:01:05.360

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000100
Data:

[0]00 00 00 04
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:1 (RNC to UE)
Message Length (bits):312
Message:

[0]80 00 00 01 02 82 07 C8
[8]80 A7 32 99 2A 3D 10 00
[16]00 05 E2 40 1E E0 00 42
[24]30 02 00 46 FF 02 22 10
[32]41 03 20 00 04 8C 00

#### CMAC Integrity Check Result

MAC RRC @ 00:01:05.360

Message Details:

Integrity Check Result:

MAC-I:10111010100011100010001011001110
Data:

[0]BA 8E 22 CE

#### MAC_DATA_REQ

RLC MAC @ 00:01:05.350

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 144

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 38 DA 48 9C DF 1A 08
[8]18 75 03 19 52 A8 9F 46
[16]88 04

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:7
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]DA 48 9C DF 1A 08 18 75
[8]03 19 52 A8 9F 46 88 04

#### MAC_DATA_REQ

RLC MAC @ 00:01:05.350

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 144

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 45 17 FE B3 10 F8 5A
[8]03 AD 20 7F 00 2D 06 00
[16]00 00

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:8
Polling bit:1 (request a status report)
Length indicator 0 (octets):11
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (11 octets):

[0]B3 10 F8 5A 03 AD 20 7F
[8]00 2D 06
Padding associated with length indicator 1 (3 octets):

[0]00 00 00

#### PHY_DATA_REQ

MAC PHY @ 00:01:05.350

BTS unit: 1:1
Channel No: 1 Name: DCH
CFN: 144

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 01 8B 4E BB B8 E8 94
[8]20 25 14 84 00 16 36 86
[16]3E D4 40 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 18 B4 EB BB 8E 89 42
[8]02 51 48 40 01 63 68 63
[16]ED 44

#### CPHY_Frame_Number_CNF

LLA RRC @ 00:01:05.360

Channel ID: DL-DPCH#1
Cell ID: 0

Message Details:

CPHY_Frame_Number_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:26

frameNumber:144

#### RLC_AM_DATA_REQ

RRC LLA @ 00:01:05.360

Channel ID: Rb2
Cell ID: -1

Message Details:

RLC_AM_DATA_REQ:

cellId:-1

routingInfo:

rB_Identity:2

confirmationRequest: (AmConfirmationRequest)

noConfirmationRequest:

aM_message:

dL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode:00000000000000000000000000000000
rrc_MessageSequenceNumber:0

message: (DL_DCCH_MessageType)

physicalChannelReconfiguration:

r3:

physicalChannelReconfiguration_r3: (PhysicalChannelReconfiguration_r3_IEs)

rrc_TransactionIdentifier:0

integrityProtectionModeInfo: Omit

cipheringModeInfo: Omit

activationTime:136

new_U_RNTI: (U_RNTI) Omit

new_C_RNTI (C_RNTI): Omit
rrc_StateIndicator:cell_DCH
utran_DRX_CycleLengthCoeff (UTRAN_DRX_CycleLengthCoefficient): Omit

cn_InformationInfo: Omit

ura_Identity: Omit

dl_CounterSynchronisationInfo: Omit

frequencyInfo:

modeSpecificInfo:

fdd: (FrequencyInfoFDD)

uarfcn_UL (UARFCN): Omit
uarfcn_DL (UARFCN):10700

maxAllowedUL_TX_Power:33

ul_ChannelRequirement: (UL_ChannelRequirementWithCPCH_SetID)

ul_DPCH_Info:

ul_DPCH_PowerControlInfo:

fdd:

dpcch_PowerOffset:-40
pc_Preamble:1
sRB_delay:7

powerControlAlgorithm:

algorithm1 (TPC_StepSizeFDD):1

modeSpecificInfo:

fdd:

scramblingCodeType:longSC
scramblingCode (UL_ScramblingCode):0
numberOfDPDCH: Omit
spreadingFactor:sf16
tfci_Existence:true
numberOfFBI_Bits: Omit
puncturingLimit:pl0_96

modeSpecificInfo:

fdd:

dl_PDSCH_Information: Omit

dl_CommonInformation:

dl_DPCH_InfoCommon:

cfnHandling:

maintain:

modeSpecificInfo:

fdd:

dl_DPCH_PowerControlInfo:

modeSpecificInfo:

fdd:

dpc_Mode:singleTPC

powerOffsetPilot_pdpdch:0

dl_rate_matching_restriction: Omit

spreadingFactorAndPilot: (SF512_AndPilot)

sfd32:

positionFixedOrFlexible:flexible
tfci_Existence:true

modeSpecificInfo:

fdd:

defaultDPCH_OffsetValue (DefaultDPCH_OffsetValueFDD):0

dpch_CompressedModeInfo:

tgp_SequenceList:

TGP_Sequence:

tgpsi:1

tgps_Status:

activate:

tgcfn:140

tgps_ConfigurationParams:

tgmp:fdd_Measurement
tgprc:0
tgsn:4
tgl1 (TGL):7
tgl2 (TGL): Omit
tgd:270
tgpl1 (TGPL):3
tgpl2 (TGPL): Omit
rpp:mode0
itp:mode0

ul_DL_Mode:

ul_and_dl:

ul (UL_CompressedModeMethod):sf_2
dl (DL_CompressedModeMethod):sf_2

dl_FrameType:dl_FrameTypeA
deltaSIR1 (DeltaSIR):2
deltaSIRAfter1 (DeltaSIR):1
deltaSIR2 (DeltaSIR): Omit
deltaSIRAfter2 (DeltaSIR): Omit
nidentifyAbort: Omit
treconfirmAbort: Omit

tx_DiversityMode:noDiversity

ssdt_Information: Omit

dl_InformationPerRL_List:

DL_InformationPerRL:

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode:100

pdsch_SHO_DCH_Info: Omit

pdsch_CodeMapping: Omit

dl_DPCH_InfoPerRL:

fdd:

pCPICH_UsageForChannelEst:mayBeUsed
dpch_FrameOffset:0

secondaryCPICH_Info: Omit

dl_ChannelisationCodeList:

DL_ChannelisationCode:

secondaryScramblingCode:5

sf_AndCodeNumber: (SF512_AndCodeNumber)

sf32:0

scramblingCodeChange: Omit

tpc_CombinationIndex:0
ssdt_CellIdentity: Omit
closedLoopTimingAdjMode: Omit

sccpch_InfoforFACH: Omit

v3a0NonCriticalExtensions: Omit

#### RLC_AM_DATA_REQ: physicalChannelReconfiguration

LLA RLC @ 00:01:05.360

Channel No: 2 Name: DCCH

Message Details:

DL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode: 10111010100011100010001011001110

rrc_MessageSequenceNumber: 4

message:

physicalChannelReconfiguration:

r3:

physicalChannelReconfiguration_r3:

rrc_TransactionIdentifier: 0

integrityProtectionModeInfo: Omitted

cipheringModeInfo: Omitted

activationTime: 136

new_U_RNTI: Omitted

new_C_RNTI: Omitted

rrc_StateIndicator: cell_DCH_RRC_StateIndicator [enum=0]

utran_DRX_CycleLengthCoeff: Omitted

cn_InformationInfo: Omitted

ura_Identity: Omitted

dl_CounterSynchronisationInfo: Omitted

frequencyInfo:

modeSpecificInfo:

fdd:

uarfcn_UL: Omitted

uarfcn_DL: 10700

maxAllowedUL_TX_Power: 33

ul_ChannelRequirement:

ul_DPCH_Info:

ul_DPCH_PowerControlInfo:

fdd:

dpcch_PowerOffset: -40

pc_Preamble: 1

sRB_delay: 7

powerControlAlgorithm:

algorithm1: 1

modeSpecificInfo:

fdd:

scramblingCodeType: longSC_ScramblingCodeType [enum=1]

scramblingCode: 0

numberOfDPDCH: Default

spreadingFactor: sf16_SpreadingFactor [enum=2]

tfci_Existence: 1

numberOfFBI_Bits: Omitted

puncturingLimit: pl0_96_PuncturingLimit [enum=14]

modeSpecificInfo:

fdd:

dl_PDSCH_Information: Omitted

dl_CommonInformation:

dl_DPCH_InfoCommon:

cfnHandling:

maintain: NULL

modeSpecificInfo:

fdd:

dl_DPCH_PowerControlInfo:

modeSpecificInfo:

fdd:

dpc_Mode: singleTPC_DPC_Mode [enum=0]

powerOffsetPilot_pdpdch: 0

dl_rate_matching_restriction: Omitted

spreadingFactorAndPilot:

sfd32: NULL

positionFixedOrFlexible: flexible_PositionFixedOrFlexible [enum=1]

tfci_Existence: 1

modeSpecificInfo:

fdd:

defaultDPCH_OffsetValue: 0

dpch_CompressedModeInfo:

tgp_SequenceList:

TGP_SequenceList.element:

tgpsi: 1

tgps_Status:

activate:

tgcfn: 140

tgps_ConfigurationParams:

tgmp: fdd_Measurement_TGMP [enum=1]

tgprc: 0

tgsn: 4

tgl1: 7

tgl2: Omitted

tgd: 270

tgpl1: 3

tgpl2: Omitted

rpp: mode0_RPP [enum=0]

itp: mode0_ITP [enum=0]

ul_DL_Mode:

ul_and_dl:

ul: sf_2_UL_CompressedModeMethod [enum=0]

dl: sf_2_DL_CompressedModeMethod [enum=1]

dl_FrameType: dl_FrameTypeA_DL_FrameType [enum=0]

deltaSIR1: 2

deltaSIRAfter1: 1

deltaSIR2: Omitted

deltaSIRAfter2: Omitted

nidentifyAbort: Omitted

treconfirmAbort: Omitted

tx_DiversityMode: noDiversity_TX_DiversityMode [enum=0]

ssdt_Information: Omitted

dl_InformationPerRL_List:

DL_InformationPerRL_List.element:

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode: 100

pdsch_SHO_DCH_Info: Omitted

pdsch_CodeMapping: Omitted

dl_DPCH_InfoPerRL:

fdd:

pCPICH_UsageForChannelEst: mayBeUsed_PCPICH_UsageForChannelEst [enum=0]

dpch_FrameOffset: 0

secondaryCPICH_Info: Omitted

dl_ChannelisationCodeList:

DL_ChannelisationCodeList.element:

secondaryScramblingCode: 5

sf_AndCodeNumber:

sf32: 0

scramblingCodeChange: Omitted

tpc_CombinationIndex: 0

ssdt_CellIdentity: Omitted

closedLoopTimingAdjMode: Omitted

sccpch_InfoforFACH: Omitted

v3a0NonCriticalExtensions: Omitted

Layer 3 SDU:

[0]DD 47 11 67 22 82 07 C8
[8]80 A7 32 99 2A 3D 10 00
[16]00 05 E2 40 1E E0 00 42
[24]30 02 00 46 FF 02 22 10
[32]41 03 20 00 04 8C 00

#### CPHY_RL_Modify_REQ

RRC LLA @ 00:01:05.380

Channel ID: DL-DPCH#1
Cell ID: 0

Message Details:

CPHY_RL_Modify_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:26

ratType:fdd

modifyMessage: (CphyRlModifyReq)

activationTime: (SS_ActivationTime)

activationCFN (ActivationTime):136

physicalChannelInfo:

dPCHInfo:

ul_DPCHInfo: (UL_DPCH_Info) Omit

dl_DPCHInfo:

dl_CommonInformation:

dl_DPCH_InfoCommon:

cfnHandling:

maintain:

modeSpecificInfo:

fdd:

dl_DPCH_PowerControlInfo:

modeSpecificInfo:

fdd:

dpc_Mode:singleTPC

powerOffsetPilot_pdpdch:0

dl_rate_matching_restriction: Omit

spreadingFactorAndPilot: (SF512_AndPilot)

sfd32:

positionFixedOrFlexible:flexible
tfci_Existence:true

modeSpecificInfo:

fdd:

defaultDPCH_OffsetValue (DefaultDPCH_OffsetValueFDD):0

dpch_CompressedModeInfo:

tgp_SequenceList:

TGP_Sequence:

tgpsi:1

tgps_Status:

activate:

tgcfn:140

tgps_ConfigurationParams:

tgmp:fdd_Measurement
tgprc:0
tgsn:4
tgl1 (TGL):7
tgl2 (TGL): Omit
tgd:270
tgpl1 (TGPL):3
tgpl2 (TGPL): Omit
rpp:mode0
itp:mode0

ul_DL_Mode:

ul_and_dl:

ul (UL_CompressedModeMethod):sf_2
dl (DL_CompressedModeMethod):sf_2

dl_FrameType:dl_FrameTypeA
deltaSIR1 (DeltaSIR):2
deltaSIRAfter1 (DeltaSIR):1
deltaSIR2 (DeltaSIR): Omit
deltaSIRAfter2 (DeltaSIR): Omit
nidentifyAbort: Omit
treconfirmAbort: Omit

tx_DiversityMode:noDiversity

ssdt_Information: Omit

dl_DPCH_InfoPerRL:

fdd:

pCPICH_UsageForChannelEst:mayBeUsed
dpch_FrameOffset:0

secondaryCPICH_Info: Omit

dl_ChannelisationCodeList:

DL_ChannelisationCode:

secondaryScramblingCode:5

sf_AndCodeNumber: (SF512_AndCodeNumber)

sf32:0

scramblingCodeChange:noCodeChange

tpc_CombinationIndex:0
ssdt_CellIdentity: Omit
closedLoopTimingAdjMode: Omit

powerOffsetOfTFCI_PO1:0
powerOffsetOfTPC_PO2:0
powerOffsetOfPILOT_PO3:0
dl_TxPower:-5
dl_TxPowerMax (DL_TxPower):15
dl_TxPowerMin (DL_TxPower):-35

#### PHY_DATA_REQ

MAC PHY @ 00:01:05.390

BTS unit: 1:1
Channel No: 1 Name: DCH
CFN: 148

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 02 51 7F E0 80 80 E9
[8]FE 20 20 02 68 02 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 25 17 FE 08 08 0E 9F
[8]E2 02 00 26 80 20 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:01:05.390

BTS unit: 1:1
Channel No: 1 Name: U_DCH
CFN: 128

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 01 D1 3F ED 55 79 DA
[8]C9 3C 80 00 00 45 55 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 1D 13 FE D5 57 9D AC
[8]93 C8 00 00 04 55 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:01:05.390

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 128

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 1D 13 FE D5 57 9D AC
[8]93 C8 00 00 04 55 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:3
Polling bit:1 (request a status report)
Length indicator 0 (octets):9
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (9 octets):

[0]D5 57 9D AC 93 C8 00 00
[8]04
Padding associated with length indicator 1 (5 octets):

[0]55 55 55 55 55

#### MAC_DATA_REQ

RLC MAC @ 00:01:05.400

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 149

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 40 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:4

#### MAC_DATA_REQ

RLC MAC @ 00:01:05.430

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 152

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 48 DD 47 11 67 22 82
[8]07 C8 80 A7 32 99 2A 3D
[16]10 00

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:9
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]DD 47 11 67 22 82 07 C8
[8]80 A7 32 99 2A 3D 10 00

#### MAC_DATA_REQ

RLC MAC @ 00:01:05.430

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 152

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 50 00 05 E2 40 1E E0
[8]00 42 30 02 00 46 FF 02
[16]22 10

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:10
Polling bit:0 (status report not requested)
Last segment, not associated with any length indicators (16 octets):

[0]00 05 E2 40 1E E0 00 42
[8]30 02 00 46 FF 02 22 10

#### MAC_DATA_REQ

RLC MAC @ 00:01:05.430

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 152

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 5D 0F FE 41 03 20 00
[8]04 8C 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:11
Polling bit:1 (request a status report)
Length indicator 0 (octets):7
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (7 octets):

[0]41 03 20 00 04 8C 00
Padding associated with length indicator 1 (7 octets):

[0]00 00 00 00 00 00 00

#### CPHY Radio Link Setup REQ

LLA PHY @ 00:01:05.430

BTS unit: 1:1
Channel No: 0 Name: D_DPCH
CFN: 152

Message Details:

Configuration Parameters:

Activation Time:136
Channel Offset:7680
Scrambling Code:1605
Symbol Rate:120k
Channelization Code:0
Adjust Time:0
Power in dBm:-45
Tx Diversity:Off
Slot Format:13
Number Of DPDCH:1

DPDCH Parameters:

Item Number 0:

Power in dBm:-45
Channelization Code:0

Radio Link Setup Flag:All

Compressed Mode Gap Information:

TGPSI:0
Method:Spreading Factor Reduction
Frame Type:Type A
Delta SIR1 (dB):2
Delta SIRafter1 (dB):1
Delta SIR2 (dB):0
Delta SIRafter2 (dB):0
TGCFN:140
TGPRC:Continuous
TGSN:4
TGL1:7
TGL2:0
TGD:0
TGPL1:3
TGPL2:0
TGPS Reconfig CFN:Not present

#### PHY_DATA_REQ

MAC PHY @ 00:01:05.430

BTS unit: 1:1
Channel No: 1 Name: DCH
CFN: 152

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]10 20 04 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]02 00 40 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### CPHY Radio Link Setup CNF

PHY LLA @ 00:01:05.430

BTS unit: 1:1
Channel No: 0 Name: D_DPCH
CFN: 152

Message Details:

#### CPHY Transport Channel Configuration REQ

LLA PHY @ 00:01:05.460

BTS unit: 1:1
Channel No: 0 Name: D_DPCH
CFN: 155

Message Details:

Configuration Parameters:

Activation Time:136
DTX Position:Flexible
Second Interleave:On
Puncture Limit:0
CCTrCH Length:2100
Number Of Transport Channels:2

Transport Channels:

Item Number 0:

Transport Channel Parameters:

Transport Channel:

Name:D_DCH
Identity:0

TTI (ms):20
EP Type:Turbo Coding
CRC Size:16
RM Attribute:150
First Interleave:On
Number Of Transport Formats:5

Transport Format Set:

Transport Format 0:

Number Of Transport Blocks:0
Transport Block Size In Bits:336

Transport Format 1:

Number Of Transport Blocks:1
Transport Block Size In Bits:336

Transport Format 2:

Number Of Transport Blocks:2
Transport Block Size In Bits:336

Transport Format 3:

Number Of Transport Blocks:3
Transport Block Size In Bits:336

Transport Format 4:

Number Of Transport Blocks:4
Transport Block Size In Bits:336

RM Maximum Length:3928

Item Number 1:

Transport Channel Parameters:

Transport Channel:

Name:D_DCH
Identity:1

TTI (ms):40
EP Type:1/3 Rate Convolutional Coding
CRC Size:16
RM Attribute:170
First Interleave:On
Number Of Transport Formats:2

Transport Format Set:

Transport Format 0:

Number Of Transport Blocks:0
Transport Block Size In Bits:148

Transport Format 1:

Number Of Transport Blocks:1
Transport Block Size In Bits:148

RM Maximum Length:544

Transport Format Combination Set:

Number Of Transport Format Combinations:10

Transport Format Combinations 0:

Transport Format:0
Transport Format:0

Transport Format Combinations 1:

Transport Format:1
Transport Format:0

Transport Format Combinations 2:

Transport Format:2
Transport Format:0

Transport Format Combinations 3:

Transport Format:3
Transport Format:0

Transport Format Combinations 4:

Transport Format:4
Transport Format:0

Transport Format Combinations 5:

Transport Format:0
Transport Format:1

Transport Format Combinations 6:

Transport Format:1
Transport Format:1

Transport Format Combinations 7:

Transport Format:2
Transport Format:1

Transport Format Combinations 8:

Transport Format:3
Transport Format:1

Transport Format Combinations 9:

Transport Format:4
Transport Format:1

#### CPHY Transport Channel Configuration CNF

PHY LLA @ 00:01:05.460

BTS unit: 1:1
Channel No: 0 Name: D_DPCH
CFN: 155

Message Details:

#### PHY_DATA_REQ

MAC PHY @ 00:01:05.470

BTS unit: 1:1
Channel No: 1 Name: DCH
CFN: 156

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 03 8D A4 89 CD F1 A0
[8]81 87 50 31 95 2A 89 F4
[16]68 80 40 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 38 DA 48 9C DF 1A 08
[8]18 75 03 19 52 A8 9F 46
[16]88 04

#### CPHY_RL_Modify_CNF

LLA RRC @ 00:01:05.490

Channel ID: DL-DPCH#1
Cell ID: 0

Message Details:

CPHY_RL_Modify_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:26

#### CPHY_RL_Modify_REQ

RRC LLA @ 00:01:05.490

Channel ID: UL-DPCH#1
Cell ID: 0

Message Details:

CPHY_RL_Modify_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:20

ratType:fdd

modifyMessage: (CphyRlModifyReq)

activationTime: (SS_ActivationTime)

activationCFN (ActivationTime):136

physicalChannelInfo:

dPCHInfo:

ul_DPCHInfo: (UL_DPCH_Info)

ul_DPCH_PowerControlInfo:

fdd:

dpcch_PowerOffset:-40
pc_Preamble:1
sRB_delay:7

powerControlAlgorithm:

algorithm1 (TPC_StepSizeFDD):1

modeSpecificInfo:

fdd:

scramblingCodeType:longSC
scramblingCode (UL_ScramblingCode):0
numberOfDPDCH: Omit
spreadingFactor:sf16
tfci_Existence:true
numberOfFBI_Bits: Omit
puncturingLimit:pl0_96

dl_DPCHInfo: Omit

#### CPHY Radio Link Setup REQ

LLA PHY @ 00:01:05.510

BTS unit: 1:1
Channel No: 0 Name: U_DPCH
CFN: 160

Message Details:

Configuration Parameters:

Activation Time:136
Channel Offset:8704
Scrambling Code:16777216
Symbol Rate:240k
Channelization Code:0
Adjust Time:0
Slot Format:0
Number Of DPDCH:1

DPDCH Parameters:

Item Number 0:

Channelization Code:4

Radio Link Setup Flag:All

Compressed Mode Gap Information:

TGPSI:0
Method:Spreading Factor Reduction
Frame Type:Type A
Delta SIR1 (dB):2
Delta SIRafter1 (dB):1
Delta SIR2 (dB):0
Delta SIRafter2 (dB):0
TGCFN:140
TGPRC:Continuous
TGSN:4
TGL1:7
TGL2:0
TGD:0
TGPL1:3
TGPL2:0
TGPS Reconfig CFN:Not present

#### PHY_DATA_REQ

MAC PHY @ 00:01:05.510

BTS unit: 1:1
Channel No: 1 Name: DCH
CFN: 160

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 04 51 7F EB 31 0F 85
[8]A0 3A D2 07 F0 02 D0 60
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 45 17 FE B3 10 F8 5A
[8]03 AD 20 7F 00 2D 06 00
[16]00 00

#### CPHY Radio Link Setup CNF

PHY LLA @ 00:01:05.510

BTS unit: 1:1
Channel No: 0 Name: U_DPCH
CFN: 160

Message Details:

#### CPHY Transport Channel Configuration REQ

LLA PHY @ 00:01:05.540

BTS unit: 1:1
Channel No: 0 Name: U_DPCH
CFN: 163

Message Details:

Configuration Parameters:

Activation Time:136
DTX Position:Flexible
Second Interleave:On
Puncture Limit:96
CCTrCH Length:2400
Number Of Transport Channels:2

Transport Channels:

Item Number 0:

Transport Channel Parameters:

Transport Channel:

Name:U_DCH
Identity:0

TTI (ms):20
EP Type:Turbo Coding
CRC Size:16
RM Attribute:150
First Interleave:On
Number Of Transport Formats:5

Transport Format Set:

Transport Format 0:

Number Of Transport Blocks:0
Transport Block Size In Bits:336

Transport Format 1:

Number Of Transport Blocks:1
Transport Block Size In Bits:336

Transport Format 2:

Number Of Transport Blocks:2
Transport Block Size In Bits:336

Transport Format 3:

Number Of Transport Blocks:3
Transport Block Size In Bits:336

Transport Format 4:

Number Of Transport Blocks:4
Transport Block Size In Bits:336

RM Maximum Length:2400

Item Number 1:

Transport Channel Parameters:

Transport Channel:

Name:U_DCH
Identity:1

TTI (ms):40
EP Type:1/3 Rate Convolutional Coding
CRC Size:16
RM Attribute:170
First Interleave:On
Number Of Transport Formats:2

Transport Format Set:

Transport Format 0:

Number Of Transport Blocks:0
Transport Block Size In Bits:148

Transport Format 1:

Number Of Transport Blocks:1
Transport Block Size In Bits:148

RM Maximum Length:291

Transport Format Combination Set:

Number Of Transport Format Combinations:10

Transport Format Combinations 0:

Transport Format:0
Transport Format:0

Transport Format Combinations 1:

Transport Format:1
Transport Format:0

Transport Format Combinations 2:

Transport Format:2
Transport Format:0

Transport Format Combinations 3:

Transport Format:3
Transport Format:0

Transport Format Combinations 4:

Transport Format:4
Transport Format:0

Transport Format Combinations 5:

Transport Format:0
Transport Format:1

Transport Format Combinations 6:

Transport Format:1
Transport Format:1

Transport Format Combinations 7:

Transport Format:2
Transport Format:1

Transport Format Combinations 8:

Transport Format:3
Transport Format:1

Transport Format Combinations 9:

Transport Format:4
Transport Format:1

#### MAC_DATA_REQ

RLC MAC @ 00:01:05.550

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 164

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 25 17 FE 08 08 0E 9F
[8]E2 02 00 26 80 20 00 00
[16]00 00

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:4
Polling bit:1 (request a status report)
Length indicator 0 (octets):11
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (11 octets):

[0]08 08 0E 9F E2 02 00 26
[8]80 20 00
Padding associated with length indicator 1 (3 octets):

[0]00 00 00

#### PHY_DATA_REQ

MAC PHY @ 00:01:05.550

BTS unit: 1:1
Channel No: 1 Name: DCH
CFN: 164

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 04 8D D4 71 16 72 28
[8]20 7C 88 0A 73 29 92 A3
[16]D1 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 48 DD 47 11 67 22 82
[8]07 C8 80 A7 32 99 2A 3D
[16]10 00

#### CPHY Transport Channel Configuration CNF

PHY LLA @ 00:01:05.550

BTS unit: 1:1
Channel No: 0 Name: U_DPCH
CFN: 164

Message Details:

#### CPHY_RL_Modify_CNF

LLA RRC @ 00:01:05.570

Channel ID: UL-DPCH#1
Cell ID: 0

Message Details:

CPHY_RL_Modify_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:20

#### PHY_DATA_REQ

MAC PHY @ 00:01:05.590

BTS unit: 1:1
Channel No: 1 Name: DCH
CFN: 168

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 05 00 00 5E 24 01 EE
[8]00 04 23 00 20 04 6F F0
[16]22 21 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 50 00 05 E2 40 1E E0
[8]00 42 30 02 00 46 FF 02
[16]22 10

#### MAC_DATA_REQ

RLC MAC @ 00:01:05.630

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 172

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 5D 0F FE 41 03 20 00
[8]04 8C 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:11
Polling bit:1 (request a status report)
Length indicator 0 (octets):7
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (7 octets):

[0]41 03 20 00 04 8C 00
Padding associated with length indicator 1 (7 octets):

[0]00 00 00 00 00 00 00

#### PHY_DATA_REQ

MAC PHY @ 00:01:05.630

BTS unit: 1:1
Channel No: 1 Name: DCH
CFN: 172

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 05 D0 FF E4 10 32 00
[8]00 48 C0 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 5D 0F FE 41 03 20 00
[8]04 8C 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_REQ

MAC PHY @ 00:01:05.670

BTS unit: 1:1
Channel No: 1 Name: DCH
CFN: 176

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]28 02 51 7F E0 80 80 E9
[8]FE 20 20 02 68 02 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]80 25 17 FE 08 08 0E 9F
[8]E2 02 00 26 80 20 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:01:05.670

BTS unit: 1:1
Channel No: 1 Name: U_DCH
CFN: 156

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 05 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 50 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### MAC_DATA_IND

MAC RLC @ 00:01:05.670

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 156

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 50 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:5

#### PHY_DATA_REQ

MAC PHY @ 00:01:05.710

BTS unit: 1:1
Channel No: 1 Name: DCH
CFN: 180

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 05 D0 FF E4 10 32 00
[8]00 48 C0 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 5D 0F FE 41 03 20 00
[8]04 8C 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:01:05.790

BTS unit: 1:1
Channel No: 1 Name: U_DCH
CFN: 168

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]10 20 09 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]02 00 90 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### MAC_DATA_IND

MAC RLC @ 00:01:05.790

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 168

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 90 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:9

#### MAC_DATA_REQ

RLC MAC @ 00:01:05.830

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 192

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 5D 0F FE 41 03 20 00
[8]04 8C 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:11
Polling bit:1 (request a status report)
Length indicator 0 (octets):7
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (7 octets):

[0]41 03 20 00 04 8C 00
Padding associated with length indicator 1 (7 octets):

[0]00 00 00 00 00 00 00

#### PHY_DATA_REQ

MAC PHY @ 00:01:05.830

BTS unit: 1:1
Channel No: 1 Name: DCH
CFN: 192

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 05 D0 FF E4 10 32 00
[8]00 48 C0 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 5D 0F FE 41 03 20 00
[8]04 8C 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:01:05.950

BTS unit: 1:1
Channel No: 1 Name: U_DCH
CFN: 184

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]20 20 05 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:2
MAC SDU (144 bits):

[0]02 00 50 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### MAC_DATA_IND

MAC RLC @ 00:01:05.950

Category: Configuration
BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 184

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 50 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:5

#### PHY_DATA_IND

PHY MAC @ 00:01:05.990

BTS unit: 1:1
Channel No: 1 Name: U_DCH
CFN: 188

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]10 20 0C 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]02 00 C0 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### MAC_DATA_IND

MAC RLC @ 00:01:05.990

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 188

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 C0 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:12

#### PHY_DATA_IND

PHY MAC @ 00:01:06.190

BTS unit: 1:1
Channel No: 1 Name: U_DCH
CFN: 208

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]10 20 0C 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]02 00 C0 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### MAC_DATA_IND

MAC RLC @ 00:01:06.190

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 208

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 C0 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:12

#### PHY_DATA_IND

PHY MAC @ 00:01:08.270

BTS unit: 1:1
Channel No: 1 Name: U_DCH
CFN: 160

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 02 50 FF E8 9F 8E C6
[8]B9 A4 00 05 55 55 55 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 25 0F FE 89 F8 EC 6B
[8]9A 40 00 55 55 55 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:01:08.270

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 160

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 25 0F FE 89 F8 EC 6B
[8]9A 40 00 55 55 55 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:4
Polling bit:1 (request a status report)
Length indicator 0 (octets):7
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (7 octets):

[0]89 F8 EC 6B 9A 40 00
Padding associated with length indicator 1 (7 octets):

[0]55 55 55 55 55 55 55

#### MAC_DATA_REQ

RLC MAC @ 00:01:08.280

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 181

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 50 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:5

#### CMAC Integrity Check Request

RRC MAC @ 00:01:08.300

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000011
Data:

[0]00 00 00 03
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:0 (UE to RNC)
Message Length (bits):56
Message:

[0]80 00 00 01 02 40 00

#### RLC_AM_DATA_IND: physicalChannelReconfigurationComplete

RLC LLA @ 00:01:08.300

Channel No: 2 Name: DCCH

Message Details:

UL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode: 00010011111100011101100011010111

rrc_MessageSequenceNumber: 3

message:

physicalChannelReconfigurationComplete:

rrc_TransactionIdentifier: 0

ul_IntegProtActivationInfo: Omitted

ul_TimingAdvance: Omitted

count_C_ActivationTime: Omitted

rb_UL_CiphActivationTimeInfo: Omitted

ul_CounterSynchronisationInfo: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]89 F8 EC 6B 9A 40 00

#### CMAC Integrity Check Result

MAC RRC @ 00:01:08.300

Message Details:

Integrity Check Result:

MAC-I:00010011111100011101100011010111
Data:

[0]13 F1 D8 D7

#### RLC_AM_DATA_IND

LLA RRC @ 00:01:08.300

Channel ID: Rb2
Cell ID: -1

Message Details:

RLC_AM_DATA_IND:

cellId:-1

routingInfo:

rB_Identity:2

integrityResult:

integrityUsed (IntegrityStatus):i_pass

aM_message:

uL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode:00010011111100011101100011010111
rrc_MessageSequenceNumber:3

message: (UL_DCCH_MessageType)

physicalChannelReconfigurationComplete:

rrc_TransactionIdentifier:0

ul_IntegProtActivationInfo: (IntegrityProtActivationInfo) Omit

ul_TimingAdvance: Omit
count_C_ActivationTime (ActivationTime): Omit

rb_UL_CiphActivationTimeInfo: (RB_ActivationTimeInfoList) Omit

ul_CounterSynchronisationInfo: Omit

laterNonCriticalExtensions: Omit

#### PHY_DATA_REQ

MAC PHY @ 00:01:08.310

BTS unit: 1:1
Channel No: 1 Name: DCH
CFN: 184

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]10 20 05 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]02 00 50 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:01:08.470

BTS unit: 1:1
Channel No: 1 Name: U_DCH
CFN: 180

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]18 02 50 FF E8 9F 8E C6
[8]B9 A4 00 05 55 55 55 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]80 25 0F FE 89 F8 EC 6B
[8]9A 40 00 55 55 55 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:01:08.470

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 180

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]80 25 0F FE 89 F8 EC 6B
[8]9A 40 00 55 55 55 55 55
[16]55 55

RLC PDU (decoded):

D/C:1 (acknowledged mode data PDU)
Sequence number:4
Polling bit:1 (request a status report)
Length indicator 0 (octets):7
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (7 octets):

[0]89 F8 EC 6B 9A 40 00
Padding associated with length indicator 1 (7 octets):

[0]55 55 55 55 55 55 55

#### MAC_DATA_REQ

RLC MAC @ 00:01:08.480

Category: Configuration
BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 201

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 00 50 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

D/C:0 (control PDU)
PDU type:0 (status)

SUFI 0:

type:2 (ack)
LSN:5

#### PHY_DATA_REQ

MAC PHY @ 00:01:08.510

BTS unit: 1:1
Channel No: 1 Name: DCH
CFN: 204

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]10 20 05 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:1
MAC SDU (144 bits):

[0]02 00 50 00 00 00 00 00
[8]00 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:01:13.350

BTS unit: 1:1
Channel No: 1 Name: U_DCH
CFN: 156

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]00 11 9F EC 62 EE 0A 08
[8]A0 46 70 15 2A 80 FA 05
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:0
MAC SDU (144 bits):

[0]01 19 FE C6 2E E0 A0 8A
[8]04 67 01 52 A8 0F A0 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:01:13.350

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 156

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]01 19 FE C6 2E E0 A0 8A
[8]04 67 01 52 A8 0F A0 55
[16]55 55

RLC PDU (decoded):

Sequence number:0
Length indicator 0 (octets):12
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (12 octets):

[0]C6 2E E0 A0 8A 04 67 01
[8]52 A8 0F A0
Padding associated with length indicator 1 (3 octets):

[0]55 55 55

#### CMAC Integrity Check Request

RRC MAC @ 00:01:13.380

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000001
Data:

[0]00 00 00 01
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:0 (UE to RNC)
Message Length (bits):96
Message:

[0]80 00 00 00 82 04 67 01
[8]52 A8 0F A0

#### RLC_UM_DATA_IND: measurementReport

RLC LLA @ 00:01:13.380

Channel No: 1 Name: DCCH

Message Details:

UL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode: 10001100010111011100000101000001

rrc_MessageSequenceNumber: 1

message:

measurementReport:

measurementIdentity: 4

measuredResults: Omitted

measuredResultsOnRACH: Omitted

additionalMeasuredResults: Omitted

eventResults:

interFreqEventResults:

eventID: e2e_EventIDInterFreq [enum=4]

interFreqCellList:

InterFreqCellList.element:

frequencyInfo:

modeSpecificInfo:

fdd:

uarfcn_UL: Omitted

uarfcn_DL: 10837

nonFreqRelatedEventResults:

fdd:

CellMeasurementEventResults.fdd.element:

primaryScramblingCode: 250

v390nonCriticalExtensions: Omitted

Layer 3 SDU:

[0]C6 2E E0 A0 8A 04 67 01
[8]52 A8 0F A0

#### CMAC Integrity Check Result

MAC RRC @ 00:01:13.380

Message Details:

Integrity Check Result:

MAC-I:10001100010111011100000101000001
Data:

[0]8C 5D C1 41

#### RLC_UM_DATA_IND

LLA RRC @ 00:01:13.380

Channel ID: Rb1
Cell ID: -1

Message Details:

RLC_UM_DATA_IND:

cellId:-1

routingInfo:

rB_Identity:1

integrityResult:

integrityUsed (IntegrityStatus):i_pass

uM_message:

uL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode:10001100010111011100000101000001
rrc_MessageSequenceNumber:1

message: (UL_DCCH_MessageType)

measurementReport:

measurementIdentity:4

measuredResults: Omit

measuredResultsOnRACH: Omit

additionalMeasuredResults: (MeasuredResultsList) Omit

eventResults:

interFreqEventResults:

eventID (EventIDInterFreq):e2e

interFreqCellList:

InterFreqCell:

frequencyInfo:

modeSpecificInfo:

fdd: (FrequencyInfoFDD)

uarfcn_UL (UARFCN): Omit
uarfcn_DL (UARFCN):10837

nonFreqRelatedEventResults: (CellMeasurementEventResults)

fdd:

PrimaryCPICH_Info:

primaryScramblingCode:250

v390nonCriticalExtensions: Omit

#### CPHY_Cell_TxPower_Modify_REQ

RRC LLA @ 00:01:13.400

Cell ID: 3

Message Details:

CPHY_Cell_TxPower_Modify_REQ:

cellId:3
dLTxAttenuationLevel:0

#### CPHY BTS Power REQ

LLA PHY @ 00:01:13.460

BTS unit: 1:2
CFN: 187

Message Details:

Configuration Parameters:

Power Control:Manual
Tx Power Step In dB:30

#### CPHY BTS Power CNF

PHY LLA @ 00:01:13.460

BTS unit: 1:2
CFN: 187

Message Details:

#### CPHY_Cell_TxPower_Modify_CNF

LLA RRC @ 00:01:13.470

Cell ID: 3

Message Details:

CPHY_Cell_TxPower_Modify_CNF:

cellId:3

#### CPHY_Cell_TxPower_Modify_REQ

RRC LLA @ 00:01:23.490

Cell ID: 0

Message Details:

CPHY_Cell_TxPower_Modify_REQ:

cellId:0
dLTxAttenuationLevel:25

#### CPHY BTS Power REQ

LLA PHY @ 00:01:23.590

BTS unit: 1:1
CFN: 176

Message Details:

Configuration Parameters:

Power Control:Manual
Tx Power Step In dB:-25

#### CPHY BTS Power CNF

PHY LLA @ 00:01:23.590

BTS unit: 1:1
CFN: 176

Message Details:

#### CPHY_Cell_TxPower_Modify_CNF

LLA RRC @ 00:01:23.630

Cell ID: 0

Message Details:

CPHY_Cell_TxPower_Modify_CNF:

cellId:0

#### PHY_DATA_IND

PHY MAC @ 00:01:29.110

BTS unit: 1:1
Channel No: 1 Name: U_DCH
CFN: 196

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]00 2B 78 AE 21 A9 22 46
[8]45 2A 55 00 27 D3 73 20
[16]A9 54 00 00

TB set (decoded):

TB 0:

C/T:0
MAC SDU (144 bits):

[0]02 B7 8A E2 1A 92 24 64
[8]52 A5 50 02 7D 37 32 0A
[16]95 40

#### MAC_DATA_IND

MAC RLC @ 00:01:29.110

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 196

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]02 B7 8A E2 1A 92 24 64
[8]52 A5 50 02 7D 37 32 0A
[16]95 40

RLC PDU (decoded):

Sequence number:1
Last segment, not associated with any length indicators (17 octets):

[0]B7 8A E2 1A 92 24 64 52
[8]A5 50 02 7D 37 32 0A 95
[16]40

#### PHY_DATA_IND

PHY MAC @ 00:01:29.150

BTS unit: 1:1
Channel No: 1 Name: U_DCH
CFN: 200

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]00 50 5F E7 D0 05 55 55
[8]55 55 55 55 55 55 55 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:0
MAC SDU (144 bits):

[0]05 05 FE 7D 00 55 55 55
[8]55 55 55 55 55 55 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:01:29.150

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 200

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]05 05 FE 7D 00 55 55 55
[8]55 55 55 55 55 55 55 55
[16]55 55

RLC PDU (decoded):

Sequence number:2
Length indicator 0 (octets):2
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (2 octets):

[0]7D 00
Padding associated with length indicator 1 (13 octets):

[0]55 55 55 55 55 55 55 55
[8]55 55 55 55 55

#### CMAC Integrity Check Request

RRC MAC @ 00:01:29.180

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000010
Data:

[0]00 00 00 02
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:0 (UE to RNC)
Message Length (bits):152
Message:

[0]80 00 00 00 82 24 64 52
[8]A5 50 02 7D 37 32 0A 95
[16]40 7D 00

#### RLC_UM_DATA_IND: measurementReport

RLC LLA @ 00:01:29.180

Channel No: 1 Name: DCCH

Message Details:

UL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode: 01101111000101011100010000110101

rrc_MessageSequenceNumber: 2

message:

measurementReport:

measurementIdentity: 4

measuredResults:

interFreqMeasuredResultsList:

InterFreqMeasuredResultsList.element:

frequencyInfo:

modeSpecificInfo:

fdd:

uarfcn_UL: Omitted

uarfcn_DL: 10837

utra_CarrierRSSI: Omitted

interFreqCellMeasuredResultsList:

InterFreqCellMeasuredResultsList.element:

cellIdentity: Omitted

dummy: Omitted

cellSynchronisationInfo: Omitted

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode: 250

cpich_Ec_N0: Omitted

cpich_RSCP: 55

pathloss: Omitted

measuredResultsOnRACH: Omitted

additionalMeasuredResults: Omitted

eventResults:

interFreqEventResults:

eventID: e2b_EventIDInterFreq [enum=1]

interFreqCellList:

InterFreqCellList.element:

frequencyInfo:

modeSpecificInfo:

fdd:

uarfcn_UL: Omitted

uarfcn_DL: 10837

nonFreqRelatedEventResults:

fdd:

CellMeasurementEventResults.fdd.element:

primaryScramblingCode: 250

v390nonCriticalExtensions: Omitted

Layer 3 SDU:

[0]B7 8A E2 1A 92 24 64 52
[8]A5 50 02 7D 37 32 0A 95
[16]40 7D 00

#### CMAC Integrity Check Result

MAC RRC @ 00:01:29.180

Message Details:

Integrity Check Result:

MAC-I:01101111000101011100010000110101
Data:

[0]6F 15 C4 35

#### RLC_UM_DATA_IND

LLA RRC @ 00:01:29.180

Channel ID: Rb1
Cell ID: -1

Message Details:

RLC_UM_DATA_IND:

cellId:-1

routingInfo:

rB_Identity:1

integrityResult:

integrityUsed (IntegrityStatus):i_pass

uM_message:

uL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode:01101111000101011100010000110101
rrc_MessageSequenceNumber:2

message: (UL_DCCH_MessageType)

measurementReport:

measurementIdentity:4

measuredResults:

interFreqMeasuredResultsList:

InterFreqMeasuredResults:

frequencyInfo:

modeSpecificInfo:

fdd: (FrequencyInfoFDD)

uarfcn_UL (UARFCN): Omit
uarfcn_DL (UARFCN):10837

utra_CarrierRSSI: Omit

interFreqCellMeasuredResultsList:

CellMeasuredResults:

cellIdentity: Omit

dummy: (SFN_SFN_ObsTimeDifference) Omit

cellSynchronisationInfo: Omit

modeSpecificInfo:

fdd:

primaryCPICH_Info:

primaryScramblingCode:250

cpich_Ec_N0: Omit
cpich_RSCP:55
pathloss: Omit

measuredResultsOnRACH: Omit

additionalMeasuredResults: (MeasuredResultsList) Omit

eventResults:

interFreqEventResults:

eventID (EventIDInterFreq):e2b

interFreqCellList:

InterFreqCell:

frequencyInfo:

modeSpecificInfo:

fdd: (FrequencyInfoFDD)

uarfcn_UL (UARFCN): Omit
uarfcn_DL (UARFCN):10837

nonFreqRelatedEventResults: (CellMeasurementEventResults)

fdd:

PrimaryCPICH_Info:

primaryScramblingCode:250

v390nonCriticalExtensions: Omit

#### CMAC Integrity Check Request

RRC MAC @ 00:01:30.190

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000001
Data:

[0]00 00 00 01
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:1 (RNC to UE)
Message Length (bits):56
Message:

[0]80 00 00 00 83 C8 00

#### CMAC Integrity Check Result

MAC RRC @ 00:01:30.190

Message Details:

Integrity Check Result:

MAC-I:11101100100111000001011111010011
Data:

[0]EC 9C 17 D3

#### RLC_UM_DATA_REQ

RRC LLA @ 00:01:30.190

Channel ID: Rb1
Cell ID: -1

Message Details:

RLC_UM_DATA_REQ:

cellId:-1

routingInfo:

rB_Identity:1

uM_message:

dL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode:00000000000000000000000000000000
rrc_MessageSequenceNumber:0

message: (DL_DCCH_MessageType)

rrcConnectionRelease:

r3:

rrcConnectionRelease_r3: (RRCConnectionRelease_r3_IEs)

rrc_TransactionIdentifier:0
n_308:1
releaseCause:normalEvent

rplmn_information: Omit

laterNonCriticalExtensions: Omit

specialLI:false

#### RLC_UM_DATA_REQ: rrcConnectionRelease

LLA RLC @ 00:01:30.190

Channel No: 1 Name: DCCH

Message Details:

DL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode: 11101100100111000001011111010011

rrc_MessageSequenceNumber: 1

message:

rrcConnectionRelease:

r3:

rrcConnectionRelease_r3:

rrc_TransactionIdentifier: 0

n_308: 1

releaseCause: normalEvent_ReleaseCause [enum=0]

rplmn_information: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]F6 4E 0B E9 8B C8 00

#### MAC_DATA_REQ

RLC MAC @ 00:01:30.310

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 80

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]01 0F FE F6 4E 0B E9 8B
[8]C8 00 00 00 00 00 00 00
[16]00 00

RLC PDU (decoded):

Sequence number:0
Length indicator 0 (octets):7
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (7 octets):

[0]F6 4E 0B E9 8B C8 00
Padding associated with length indicator 1 (8 octets):

[0]00 00 00 00 00 00 00 00

#### PHY_DATA_REQ

MAC PHY @ 00:01:30.310

BTS unit: 1:1
Channel No: 1 Name: DCH
CFN: 80

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]00 10 FF EF 64 E0 BE 98
[8]BC 80 00 00 00 00 00 00
[16]00 00 00 00

TB set (decoded):

TB 0:

C/T:0
MAC SDU (144 bits):

[0]01 0F FE F6 4E 0B E9 8B
[8]C8 00 00 00 00 00 00 00
[16]00 00

#### PHY_DATA_IND

PHY MAC @ 00:01:30.590

BTS unit: 1:1
Channel No: 1 Name: U_DCH
CFN: 88

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]00 70 DF EB 1E 34 8C 21
[8]C4 05 55 55 55 55 55 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:0
MAC SDU (144 bits):

[0]07 0D FE B1 E3 48 C2 1C
[8]40 55 55 55 55 55 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:01:30.590

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 88

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]07 0D FE B1 E3 48 C2 1C
[8]40 55 55 55 55 55 55 55
[16]55 55

RLC PDU (decoded):

Sequence number:3
Length indicator 0 (octets):6
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (6 octets):

[0]B1 E3 48 C2 1C 40
Padding associated with length indicator 1 (9 octets):

[0]55 55 55 55 55 55 55 55
[8]55

#### CMAC Integrity Check Request

RRC MAC @ 00:01:30.620

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000011
Data:

[0]00 00 00 03
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:0 (UE to RNC)
Message Length (bits):48
Message:

[0]80 00 00 00 84 40

#### RLC_UM_DATA_IND: rrcConnectionReleaseComplete

RLC LLA @ 00:01:30.620

Channel No: 1 Name: DCCH

Message Details:

UL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode: 01100011110001101001000110000100

rrc_MessageSequenceNumber: 3

message:

rrcConnectionReleaseComplete:

rrc_TransactionIdentifier: 0

errorIndication: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]B1 E3 48 C2 1C 40

#### CMAC Integrity Check Result

MAC RRC @ 00:01:30.620

Message Details:

Integrity Check Result:

MAC-I:01100011110001101001000110000100
Data:

[0]63 C6 91 84

#### RLC_UM_DATA_IND

LLA RRC @ 00:01:30.620

Channel ID: Rb1
Cell ID: -1

Message Details:

RLC_UM_DATA_IND:

cellId:-1

routingInfo:

rB_Identity:1

integrityResult:

integrityUsed (IntegrityStatus):i_pass

uM_message:

uL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode:01100011110001101001000110000100
rrc_MessageSequenceNumber:3

message: (UL_DCCH_MessageType)

rrcConnectionReleaseComplete:

rrc_TransactionIdentifier:0

errorIndication: (FailureCauseWithProtErr) Omit

laterNonCriticalExtensions: Omit

#### PHY_DATA_IND

PHY MAC @ 00:01:30.750

BTS unit: 1:1
Channel No: 1 Name: U_DCH
CFN: 104

Message Details:

TFI:1
TB set size:148
TB size:148
TB set (raw):

[0]00 90 DF E9 59 7C B1 72
[8]44 05 55 55 55 55 55 55
[16]55 55 50 00

TB set (decoded):

TB 0:

C/T:0
MAC SDU (144 bits):

[0]09 0D FE 95 97 CB 17 24
[8]40 55 55 55 55 55 55 55
[16]55 55

#### MAC_DATA_IND

MAC RLC @ 00:01:30.750

Category: Configuration
BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 104

Message Details:

RLC PDU size (bits):144
RLC PDU (raw):

[0]09 0D FE 95 97 CB 17 24
[8]40 55 55 55 55 55 55 55
[16]55 55

RLC PDU (decoded):

Sequence number:4
Length indicator 0 (octets):6
Length indicator 1 (octets):127 (padding)
Segment associated with length indicator 0 (6 octets):

[0]95 97 CB 17 24 40
Padding associated with length indicator 1 (9 octets):

[0]55 55 55 55 55 55 55 55
[8]55

#### CMAC Integrity Check Request

RRC MAC @ 00:01:30.790

Message Details:

Integrity Check Parameters:

IntegrityKey:01110111011001100001000100000000001100110010001011011101110011001111111111101110100110011000100010111011101010100101010101000100
Data:

[0]77 66 11 00 33 22 DD CC
[8]FF EE 99 88 BB AA 55 44
Count I:00000000000000000000000000000100
Data:

[0]00 00 00 04
Fresh:00001111000011110000111100001111
Data:

[0]0F 0F 0F 0F
Direction:0 (UE to RNC)
Message Length (bits):48
Message:

[0]80 00 00 00 84 40

#### RLC_UM_DATA_IND: rrcConnectionReleaseComplete

RLC LLA @ 00:01:30.790

Channel No: 1 Name: DCCH

Message Details:

UL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode: 00101011001011111001011000101110

rrc_MessageSequenceNumber: 4

message:

rrcConnectionReleaseComplete:

rrc_TransactionIdentifier: 0

errorIndication: Omitted

laterNonCriticalExtensions: Omitted

Layer 3 SDU:

[0]95 97 CB 17 24 40

#### CMAC Integrity Check Result

MAC RRC @ 00:01:30.790

Message Details:

Integrity Check Result:

MAC-I:00101011001011111001011000101110
Data:

[0]2B 2F 96 2E

#### RLC_UM_DATA_IND

LLA RRC @ 00:01:30.790

Channel ID: Rb1
Cell ID: -1

Message Details:

RLC_UM_DATA_IND:

cellId:-1

routingInfo:

rB_Identity:1

integrityResult:

integrityUsed (IntegrityStatus):i_pass

uM_message:

uL_DCCH_Message:

integrityCheckInfo:

messageAuthenticationCode:00101011001011111001011000101110
rrc_MessageSequenceNumber:4

message: (UL_DCCH_MessageType)

rrcConnectionReleaseComplete:

rrc_TransactionIdentifier:0

errorIndication: (FailureCauseWithProtErr) Omit

laterNonCriticalExtensions: Omit

#### CRLC_Config_REQ

RRC LLA @ 00:01:30.790

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:1

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CPHY_OUTSYNC_IND

PHY RRC @ 00:01:30.810

BTS unit: 1:1
Channel No: 0 Name: U_DPCH
CFN: 130

Message Details:

#### CRLC UM Channel Release REQ

LLA RLC @ 00:01:30.950

BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 144

Message Details:

#### CRLC UM Channel Release CNF

RLC LLA @ 00:01:30.950

BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 144

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:01:30.960

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:1

#### CRLC_Config_REQ

RRC LLA @ 00:01:30.960

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:2

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC AM Channel Release REQ

LLA RLC @ 00:01:31.010

BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 150

Message Details:

#### CRLC AM Channel Release CNF

RLC LLA @ 00:01:31.010

BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 150

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:01:31.020

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:2

#### CRLC_Config_REQ

RRC LLA @ 00:01:31.020

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:3

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC AM Channel Release REQ

LLA RLC @ 00:01:31.110

BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 160

Message Details:

#### CRLC AM Channel Release CNF

RLC LLA @ 00:01:31.110

BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 160

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:01:31.130

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:3

#### CRLC_Config_REQ

RRC LLA @ 00:01:31.130

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:4

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC AM Channel Release REQ

LLA RLC @ 00:01:31.220

BTS unit: 1:1
Channel No: 4 Name: DCCH
CFN: 171

Message Details:

#### CRLC AM Channel Release CNF

RLC LLA @ 00:01:31.220

BTS unit: 1:1
Channel No: 4 Name: DCCH
CFN: 171

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:01:31.240

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:4

#### CRLC_Config_REQ

RRC LLA @ 00:01:31.240

Channel ID: Rb20
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:20

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC AM Channel Release REQ

LLA RLC @ 00:01:31.270

BTS unit: 1:1
Channel No: 4 Name: D_DTCH
CFN: 176

Message Details:

#### CRLC AM Channel Release CNF

RLC LLA @ 00:01:31.280

BTS unit: 1:1
Channel No: 4 Name: D_DTCH
CFN: 177

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:01:31.290

Channel ID: Rb20
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:20

#### CMAC_Config_REQ

RRC LLA @ 00:01:31.290

Channel ID: DL-DPCH#1
Cell ID: -1

Message Details:

CMAC_Config_REQ:

cellId:-1

routingInfo:

physicalChannelIdentity:26

ratType:fdd

configMessage:

release:

#### CMAC Configuration REQ

LLA MAC @ 00:01:31.310

BTS unit: 1:1
Channel No: 0 Name: D_DPCH
CFN: 180

Message Details:

Configuration Parameters:

Number Of Transport Channels:0
Active Flag:0

Transport Format Combination Set:

Number Of Transport Format Combinations:0

#### CMAC Configuration CNF

MAC LLA @ 00:01:31.310

BTS unit: 1:1
Channel No: 0 Name: D_DPCH
CFN: 180

Message Details:

#### CMAC_Config_CNF

LLA RRC @ 00:01:31.330

Channel ID: DL-DPCH#1
Cell ID: -1

Message Details:

CMAC_Config_CNF:

cellId:-1

routingInfo:

physicalChannelIdentity:26

#### CMAC_Config_REQ

RRC LLA @ 00:01:31.330

Channel ID: UL-DPCH#1
Cell ID: -1

Message Details:

CMAC_Config_REQ:

cellId:-1

routingInfo:

physicalChannelIdentity:20

ratType:fdd

configMessage:

release:

#### CMAC Configuration REQ

LLA MAC @ 00:01:31.350

BTS unit: 1:1
Channel No: 0 Name: U_DPCH
CFN: 184

Message Details:

Configuration Parameters:

Number Of Transport Channels:0
Active Flag:0

Transport Format Combination Set:

Number Of Transport Format Combinations:0

#### CMAC Configuration CNF

MAC LLA @ 00:01:31.350

BTS unit: 1:1
Channel No: 0 Name: U_DPCH
CFN: 184

Message Details:

#### CMAC_Config_CNF

LLA RRC @ 00:01:31.370

Channel ID: UL-DPCH#1
Cell ID: -1

Message Details:

CMAC_Config_CNF:

cellId:-1

routingInfo:

physicalChannelIdentity:20

#### CPHY_TrCH_Release_REQ

RRC LLA @ 00:01:31.370

Channel ID: DL-DPCH#1
Cell ID: 0

Message Details:

CPHY_TrCH_Release_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:26

trchConfigType:

dch:Normal

#### CPHY Transport Channel Release REQ

LLA PHY @ 00:01:31.380

BTS unit: 1:1
Channel No: 0 Name: D_DPCH
CFN: 187

Message Details:

#### CPHY Transport Channel Release CNF

PHY LLA @ 00:01:31.380

BTS unit: 1:1
Channel No: 0 Name: D_DPCH
CFN: 187

Message Details:

#### CPHY_TrCH_Release_CNF

LLA RRC @ 00:01:31.400

Channel ID: DL-DPCH#1
Cell ID: 0

Message Details:

CPHY_TrCH_Release_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:26

#### CPHY_TrCH_Release_REQ

RRC LLA @ 00:01:31.400

Channel ID: UL-DPCH#1
Cell ID: 0

Message Details:

CPHY_TrCH_Release_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:20

trchConfigType:

dch:Normal

#### CPHY Transport Channel Release REQ

LLA PHY @ 00:01:31.410

BTS unit: 1:1
Channel No: 0 Name: U_DPCH
CFN: 190

Message Details:

#### CPHY Transport Channel Release CNF

PHY LLA @ 00:01:31.410

BTS unit: 1:1
Channel No: 0 Name: U_DPCH
CFN: 190

Message Details:

#### CPHY_TrCH_Release_CNF

LLA RRC @ 00:01:31.430

Channel ID: UL-DPCH#1
Cell ID: 0

Message Details:

CPHY_TrCH_Release_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:20

#### CPHY_RL_Release_REQ

RRC LLA @ 00:01:31.430

Channel ID: DL-DPCH#1
Cell ID: 0

Message Details:

CPHY_RL_Release_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:26

#### CPHY Radio Link Release REQ

LLA PHY @ 00:01:31.440

BTS unit: 1:1
Channel No: 0 Name: D_DPCH
CFN: 193

Message Details:

#### CPHY Radio Link Release CNF

PHY LLA @ 00:01:31.440

BTS unit: 1:1
Channel No: 0 Name: D_DPCH
CFN: 193

Message Details:

#### CPHY_RL_Release_CNF

LLA RRC @ 00:01:31.460

Channel ID: DL-DPCH#1
Cell ID: 0

Message Details:

CPHY_RL_Release_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:26

#### CPHY_RL_Release_REQ

RRC LLA @ 00:01:31.460

Channel ID: UL-DPCH#1
Cell ID: 0

Message Details:

CPHY_RL_Release_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:20

#### CPHY Radio Link Release REQ

LLA PHY @ 00:01:31.470

BTS unit: 1:1
Channel No: 0 Name: U_DPCH
CFN: 196

Message Details:

#### CPHY Radio Link Release CNF

PHY LLA @ 00:01:31.470

BTS unit: 1:1
Channel No: 0 Name: U_DPCH
CFN: 196

Message Details:

#### CPHY_RL_Release_CNF

LLA RRC @ 00:01:31.490

Channel ID: UL-DPCH#1
Cell ID: 0

Message Details:

CPHY_RL_Release_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:20

#### CPHY_RL_Setup_REQ

RRC LLA @ 00:01:31.490

Channel ID: DL-DPCH#1
Cell ID: 0

Message Details:

CPHY_RL_Setup_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:26

ratType:fdd

setupMessage: (CphyRlSetupReq)

physicalChannelInfo:

dPCHInfo:

ul_DPCHInfo: (UL_DPCH_Info) Omit

dl_DPCHInfo:

dl_CommonInformation:

dl_DPCH_InfoCommon:

cfnHandling:

initialise:

cfntargetsfnframeoffset: Omit

modeSpecificInfo:

fdd:

dl_DPCH_PowerControlInfo:

modeSpecificInfo:

fdd:

dpc_Mode:singleTPC

powerOffsetPilot_pdpdch:0

dl_rate_matching_restriction: Omit

spreadingFactorAndPilot: (SF512_AndPilot)

sfd128 (PilotBits128):pb4

positionFixedOrFlexible:fixed
tfci_Existence:false

modeSpecificInfo:

fdd:

defaultDPCH_OffsetValue (DefaultDPCH_OffsetValueFDD):0

dpch_CompressedModeInfo: Omit

tx_DiversityMode:noDiversity

ssdt_Information: Omit

dl_DPCH_InfoPerRL:

fdd:

pCPICH_UsageForChannelEst:mayBeUsed
dpch_FrameOffset:0

secondaryCPICH_Info: Omit

dl_ChannelisationCodeList:

DL_ChannelisationCode:

secondaryScramblingCode:1

sf_AndCodeNumber: (SF512_AndCodeNumber)

sf128:0

scramblingCodeChange: Omit

tpc_CombinationIndex:0
ssdt_CellIdentity: Omit
closedLoopTimingAdjMode: Omit

powerOffsetOfTFCI_PO1:0
powerOffsetOfTPC_PO2:0
powerOffsetOfPILOT_PO3:0
dl_TxPower:-5
dl_TxPowerMax (DL_TxPower):15
dl_TxPowerMin (DL_TxPower):-35

#### CPHY Radio Link Setup REQ

LLA PHY @ 00:01:31.590

BTS unit: 1:1
Channel No: 0 Name: D_DPCH
CFN: 208

Message Details:

Configuration Parameters:

Channel Offset:7680
Scrambling Code:1601
Symbol Rate:30k
Channelization Code:0
Adjust Time:0
Power in dBm:-70
Tx Diversity:Off
Slot Format:8
Number Of DPDCH:1

DPDCH Parameters:

Item Number 0:

Power in dBm:-45
Channelization Code:0

#### CPHY Radio Link Setup CNF

PHY LLA @ 00:01:31.590

BTS unit: 1:1
Channel No: 0 Name: D_DPCH
CFN: 208

Message Details:

#### CPHY_RL_Setup_CNF

LLA RRC @ 00:01:31.630

Channel ID: DL-DPCH#1
Cell ID: 0

Message Details:

CPHY_RL_Setup_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:26

#### CPHY_TrCH_Config_REQ

RRC LLA @ 00:01:31.630

Channel ID: DL-DPCH#1
Cell ID: 0

Message Details:

CPHY_TrCH_Config_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:26

ratType:fdd

trchConfigType:

dch:Normal

configMessage: (CphyTrchConfigReq)

activationTime: (SS_ActivationTime)

activateNow:

ulconnectedTrCHList: Omit

ulTFCS: (TFCS) Omit

dlconnectedTrCHList:

:

trchid (TransportChannelIdentity):10
dl_TransportChannelType (SS_DL_TransportChannelType):dch

transportChannelInfo: (CommonOrDedicatedTFS)

tti:

tti10: (CommonOrDedicatedTF_InfoList)

CommonOrDedicatedTF_Info:

tb_Size:148

numberOfTbSizeList:

NumberOfTransportBlocks:

zero:

NumberOfTransportBlocks:

one:

logicalChannelList:

allSizes:

semistaticTF_Information:

channelCodingType:

convolutional (CodingRate):third

rateMatchingAttribute:192
crc_Size:crc16

dlTFCS: (TFCS)

normalTFCI_Signalling: (ExplicitTFCS_Configuration)

complete: (TFCS_ReconfAdd)

ctfcSize:

ctfc2Bit:

:

ctfc2:0

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc2:1

powerOffsetInformation:

gainFactorInformation:

signalledGainFactors:

modeSpecificInfo:

fdd:

gainFactorBetaC (GainFactor):11

gainFactorBetaD (GainFactor):15
referenceTFC_ID:0

powerOffsetPp_m: Omit

#### CPHY Transport Channel Configuration REQ

LLA PHY @ 00:01:31.650

BTS unit: 1:1
Channel No: 0 Name: D_DPCH
CFN: 214

Message Details:

Configuration Parameters:

DTX Position:Fixed
Second Interleave:On
Puncture Limit:0
CCTrCH Length:510
Number Of Transport Channels:1

Transport Channels:

Item Number 0:

Transport Channel Parameters:

Transport Channel:

Name:D_DCH
Identity:0

TTI (ms):10
EP Type:1/3 Rate Convolutional Coding
CRC Size:16
RM Attribute:192
First Interleave:On
Number Of Transport Formats:2

Transport Format Set:

Transport Format 0:

Number Of Transport Blocks:0
Transport Block Size In Bits:148

Transport Format 1:

Number Of Transport Blocks:1
Transport Block Size In Bits:148

RM Maximum Length:510

Transport Format Combination Set:

Number Of Transport Format Combinations:2

Transport Format Combinations 0:

Transport Format:0

Transport Format Combinations 1:

Transport Format:1

#### CPHY Transport Channel Configuration CNF

PHY LLA @ 00:01:31.650

BTS unit: 1:1
Channel No: 0 Name: D_DPCH
CFN: 214

Message Details:

#### CPHY_TrCH_Config_CNF

LLA RRC @ 00:01:31.660

Channel ID: DL-DPCH#1
Cell ID: 0

Message Details:

CPHY_TrCH_Config_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:26

#### CMAC_Config_REQ

RRC LLA @ 00:01:31.660

Channel ID: DL-DPCH#1
Cell ID: -1

Message Details:

CMAC_Config_REQ:

cellId:-1

routingInfo:

physicalChannelIdentity:26

ratType:fdd

configMessage:

setup: (CmacConfigReq)

activationTime: (SS_ActivationTime)

activateNow:

uE_Info:

u_RNTI: Omit

c_RNTI: Omit

trCHInfo:

ulconnectedTrCHList: Omit

ulTFCS: (TFCS) Omit

dlconnectedTrCHList:

:

trchid (TransportChannelIdentity):10

transportChannelInfo: (CommonOrDedicatedTFS)

tti:

tti10: (CommonOrDedicatedTF_InfoList)

CommonOrDedicatedTF_Info:

tb_Size:148

numberOfTbSizeList:

NumberOfTransportBlocks:

zero:

NumberOfTransportBlocks:

one:

logicalChannelList:

allSizes:

semistaticTF_Information:

channelCodingType:

convolutional (CodingRate):third

rateMatchingAttribute:192
crc_Size:crc16

dlTFCS: (TFCS)

normalTFCI_Signalling: (ExplicitTFCS_Configuration)

complete: (TFCS_ReconfAdd)

ctfcSize:

ctfc2Bit:

:

ctfc2:0

powerOffsetInformation:

gainFactorInformation:

computedGainFactors (ReferenceTFC_ID):0

powerOffsetPp_m: Omit

:

ctfc2:1

powerOffsetInformation:

gainFactorInformation:

signalledGainFactors:

modeSpecificInfo:

fdd:

gainFactorBetaC (GainFactor):11

gainFactorBetaD (GainFactor):15
referenceTFC_ID:0

powerOffsetPp_m: Omit

trCH_LogCHMapping: (TrCH_LogCHMappingList1)

ulconnectedTrCHList: Omit

dlconnectedTrCHList:

:

trchid (TransportChannelIdentity):10

trCH_LogCHMappingList:

TrCH_LogicalChannelMapping:

logicalChannel_Mapping:

dl_LogicalChannelMapping: (SS_DL_LogicalChannelMapping)

macHeaderManipulation (MAC_HeaderManipulation):normalMacHeader
dl_TransportChannelType (SS_DL_TransportChannelType):dch
logicalChannelIdentity:1
logicalChannelType:dCCH

rlc_SizeList:

configured:

mac_LogicalChannelPriority:1

rB_Identity:1
cn_DomainIdentity: Omit

TrCH_LogicalChannelMapping:

logicalChannel_Mapping:

dl_LogicalChannelMapping: (SS_DL_LogicalChannelMapping)

macHeaderManipulation (MAC_HeaderManipulation):normalMacHeader
dl_TransportChannelType (SS_DL_TransportChannelType):dch
logicalChannelIdentity:2
logicalChannelType:dCCH

rlc_SizeList:

configured:

mac_LogicalChannelPriority:2

rB_Identity:2
cn_DomainIdentity: Omit

TrCH_LogicalChannelMapping:

logicalChannel_Mapping:

dl_LogicalChannelMapping: (SS_DL_LogicalChannelMapping)

macHeaderManipulation (MAC_HeaderManipulation):normalMacHeader
dl_TransportChannelType (SS_DL_TransportChannelType):dch
logicalChannelIdentity:3
logicalChannelType:dCCH

rlc_SizeList:

configured:

mac_LogicalChannelPriority:3

rB_Identity:3
cn_DomainIdentity: Omit

TrCH_LogicalChannelMapping:

logicalChannel_Mapping:

dl_LogicalChannelMapping: (SS_DL_LogicalChannelMapping)

macHeaderManipulation (MAC_HeaderManipulation):normalMacHeader
dl_TransportChannelType (SS_DL_TransportChannelType):dch
logicalChannelIdentity:4
logicalChannelType:dCCH

rlc_SizeList:

configured:

mac_LogicalChannelPriority:4

rB_Identity:4
cn_DomainIdentity: Omit

#### CMAC Configuration REQ

LLA MAC @ 00:01:31.680

BTS unit: 1:1
Channel No: 0 Name: D_DPCH
CFN: 217

Message Details:

Configuration Parameters:

Number Of Transport Channels:1

Transport Channels:

Item Number 0:

Transport Channel Parameters:

Transport Channel:

Name:D_DCH
Identity:0

TTI (ms):10
EP Type:1/3 Rate Convolutional Coding
CRC Size:16
RM Attribute:192
First Interleave:On
Number Of Transport Formats:2

Transport Format Set:

Transport Format 0:

Number Of Transport Blocks:0
Transport Block Size In Bits:148

Transport Format 1:

Number Of Transport Blocks:1
Transport Block Size In Bits:148

Number Of Logical Channels:4

Logical Channels:

Item Number 0:

Logical Channel:

Name:DCCH
Identity:1

Priority:1
CT Length:4
CT Value:0
TCTF Length:0
TCTF Value:0
UE ID Type:Not used
UE ID:0

Item Number 1:

Logical Channel:

Name:DCCH
Identity:2

Priority:2
CT Length:4
CT Value:1
TCTF Length:0
TCTF Value:0
UE ID Type:Not used
UE ID:0

Item Number 2:

Logical Channel:

Name:DCCH
Identity:3

Priority:3
CT Length:4
CT Value:2
TCTF Length:0
TCTF Value:0
UE ID Type:Not used
UE ID:0

Item Number 3:

Logical Channel:

Name:DCCH
Identity:4

Priority:4
CT Length:4
CT Value:3
TCTF Length:0
TCTF Value:0
UE ID Type:Not used
UE ID:0

Active Flag:1

Transport Format Combination Set:

Number Of Transport Format Combinations:2

Transport Format Combinations 0:

Transport Format:0

Transport Format Combinations 1:

Transport Format:1

#### CMAC Configuration CNF

MAC LLA @ 00:01:31.680

BTS unit: 1:1
Channel No: 0 Name: D_DPCH
CFN: 217

Message Details:

#### CMAC_Config_CNF

LLA RRC @ 00:01:31.690

Channel ID: DL-DPCH#1
Cell ID: -1

Message Details:

CMAC_Config_CNF:

cellId:-1

routingInfo:

physicalChannelIdentity:26

#### CPHY_RL_Setup_REQ

RRC LLA @ 00:01:31.690

Channel ID: UL-DPCH#1
Cell ID: 0

Message Details:

CPHY_RL_Setup_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:20

ratType:fdd

setupMessage: (CphyRlSetupReq)

physicalChannelInfo:

dPCHInfo:

ul_DPCHInfo: (UL_DPCH_Info)

ul_DPCH_PowerControlInfo:

fdd:

dpcch_PowerOffset:-40
pc_Preamble:1
sRB_delay:7

powerControlAlgorithm:

algorithm1 (TPC_StepSizeFDD):1

modeSpecificInfo:

fdd:

scramblingCodeType:longSC
scramblingCode (UL_ScramblingCode):0
numberOfDPDCH: Omit
spreadingFactor:sf64
tfci_Existence:true
numberOfFBI_Bits: Omit
puncturingLimit:pl1

dl_DPCHInfo: Omit

#### CPHY_RL_Setup_CNF

LLA RRC @ 00:01:31.710

Channel ID: UL-DPCH#1
Cell ID: 0

Message Details:

CPHY_RL_Setup_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:20

#### CPHY_TrCH_Config_REQ

RRC LLA @ 00:01:31.710

Channel ID: UL-DPCH#1
Cell ID: 0

Message Details:

CPHY_TrCH_Config_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:20

ratType:fdd

trchConfigType:

dch:Normal

configMessage: (CphyTrchConfigReq)

activationTime: (SS_ActivationTime)

activateNow:

ulconnectedTrCHList:

:

trchid (TransportChannelIdentity):5
ul_TransportChannelType (SS_UL_TransportChannelType):dch

transportChannelInfo: (CommonOrDedicatedTFS)

tti:

tti10: (CommonOrDedicatedTF_InfoList)

CommonOrDedicatedTF_Info:

tb_Size:148

numberOfTbSizeList:

NumberOfTransportBlocks:

zero:

NumberOfTransportBlocks:

one:

logicalChannelList:

allSizes:

semistaticTF_Information:

channelCodingType:

convolutional (CodingRate):third

rateMatchingAttribute:192
crc_Size:crc16

ulTFCS: (TFCS)

normalTFCI_Signalling: (ExplicitTFCS_Configuration)

complete: (TFCS_ReconfAdd)

ctfcSize:

ctfc2Bit:

:

ctfc2:0

powerOffsetInformation: Omit

:

ctfc2:1

powerOffsetInformation: Omit

dlconnectedTrCHList: Omit

dlTFCS: (TFCS) Omit

#### CPHY Radio Link Setup REQ

LLA PHY @ 00:01:31.750

BTS unit: 1:1
Channel No: 0 Name: U_DPCH
CFN: 224

Message Details:

Configuration Parameters:

Channel Offset:8704
Scrambling Code:16777216
Symbol Rate:60k
Channelization Code:0
Adjust Time:0
Slot Format:0
Number Of DPDCH:1

DPDCH Parameters:

Item Number 0:

Channelization Code:16

#### CPHY Radio Link Setup CNF

PHY LLA @ 00:01:31.750

BTS unit: 1:1
Channel No: 0 Name: U_DPCH
CFN: 224

Message Details:

#### CPHY Transport Channel Configuration REQ

LLA PHY @ 00:01:31.790

BTS unit: 1:1
Channel No: 0 Name: U_DPCH
CFN: 228

Message Details:

Configuration Parameters:

DTX Position:Flexible
Second Interleave:On
Puncture Limit:100
CCTrCH Length:600
Number Of Transport Channels:1

Transport Channels:

Item Number 0:

Transport Channel Parameters:

Transport Channel:

Name:U_DCH
Identity:0

TTI (ms):10
EP Type:1/3 Rate Convolutional Coding
CRC Size:16
RM Attribute:192
First Interleave:On
Number Of Transport Formats:2

Transport Format Set:

Transport Format 0:

Number Of Transport Blocks:0
Transport Block Size In Bits:148

Transport Format 1:

Number Of Transport Blocks:1
Transport Block Size In Bits:148

RM Maximum Length:600

Transport Format Combination Set:

Number Of Transport Format Combinations:2

Transport Format Combinations 0:

Transport Format:0

Transport Format Combinations 1:

Transport Format:1

#### CPHY Transport Channel Configuration CNF

PHY LLA @ 00:01:31.810

BTS unit: 1:1
Channel No: 0 Name: U_DPCH
CFN: 230

Message Details:

#### CPHY_TrCH_Config_CNF

LLA RRC @ 00:01:31.850

Channel ID: UL-DPCH#1
Cell ID: 0

Message Details:

CPHY_TrCH_Config_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:20

#### CMAC_Config_REQ

RRC LLA @ 00:01:31.850

Channel ID: UL-DPCH#1
Cell ID: -1

Message Details:

CMAC_Config_REQ:

cellId:-1

routingInfo:

physicalChannelIdentity:20

ratType:fdd

configMessage:

setup: (CmacConfigReq)

activationTime: (SS_ActivationTime)

activateNow:

uE_Info:

u_RNTI: Omit

c_RNTI: Omit

trCHInfo:

ulconnectedTrCHList:

:

trchid (TransportChannelIdentity):5

transportChannelInfo: (CommonOrDedicatedTFS)

tti:

tti10: (CommonOrDedicatedTF_InfoList)

CommonOrDedicatedTF_Info:

tb_Size:148

numberOfTbSizeList:

NumberOfTransportBlocks:

zero:

NumberOfTransportBlocks:

one:

logicalChannelList:

allSizes:

semistaticTF_Information:

channelCodingType:

convolutional (CodingRate):third

rateMatchingAttribute:192
crc_Size:crc16

ulTFCS: (TFCS)

normalTFCI_Signalling: (ExplicitTFCS_Configuration)

complete: (TFCS_ReconfAdd)

ctfcSize:

ctfc2Bit:

:

ctfc2:0

powerOffsetInformation: Omit

:

ctfc2:1

powerOffsetInformation: Omit

dlconnectedTrCHList: Omit

dlTFCS: (TFCS) Omit

trCH_LogCHMapping: (TrCH_LogCHMappingList1)

ulconnectedTrCHList:

:

trchid (TransportChannelIdentity):5

trCH_LogCHMappingList:

TrCH_LogicalChannelMapping:

logicalChannel_Mapping:

ul_LogicalChannelMapping: (SS_UL_LogicalChannelMapping)

macHeaderManipulation (MAC_HeaderManipulation):normalMacHeader
ul_TransportChannelType (SS_UL_TransportChannelType):dch
logicalChannelIdentity:1
logicalChannelType:dCCH

rB_Identity:1
cn_DomainIdentity: Omit

TrCH_LogicalChannelMapping:

logicalChannel_Mapping:

ul_LogicalChannelMapping: (SS_UL_LogicalChannelMapping)

macHeaderManipulation (MAC_HeaderManipulation):normalMacHeader
ul_TransportChannelType (SS_UL_TransportChannelType):dch
logicalChannelIdentity:2
logicalChannelType:dCCH

rB_Identity:2
cn_DomainIdentity: Omit

TrCH_LogicalChannelMapping:

logicalChannel_Mapping:

ul_LogicalChannelMapping: (SS_UL_LogicalChannelMapping)

macHeaderManipulation (MAC_HeaderManipulation):normalMacHeader
ul_TransportChannelType (SS_UL_TransportChannelType):dch
logicalChannelIdentity:3
logicalChannelType:dCCH

rB_Identity:3
cn_DomainIdentity: Omit

TrCH_LogicalChannelMapping:

logicalChannel_Mapping:

ul_LogicalChannelMapping: (SS_UL_LogicalChannelMapping)

macHeaderManipulation (MAC_HeaderManipulation):normalMacHeader
ul_TransportChannelType (SS_UL_TransportChannelType):dch
logicalChannelIdentity:4
logicalChannelType:dCCH

rB_Identity:4
cn_DomainIdentity: Omit

dlconnectedTrCHList: Omit

#### CMAC Configuration REQ

LLA MAC @ 00:01:31.870

BTS unit: 1:1
Channel No: 0 Name: U_DPCH
CFN: 236

Message Details:

Configuration Parameters:

Number Of Transport Channels:1

Transport Channels:

Item Number 0:

Transport Channel Parameters:

Transport Channel:

Name:U_DCH
Identity:0

TTI (ms):10
EP Type:1/3 Rate Convolutional Coding
CRC Size:16
RM Attribute:192
First Interleave:On
Number Of Transport Formats:2

Transport Format Set:

Transport Format 0:

Number Of Transport Blocks:0
Transport Block Size In Bits:148

Transport Format 1:

Number Of Transport Blocks:1
Transport Block Size In Bits:148

Number Of Logical Channels:4

Logical Channels:

Item Number 0:

Logical Channel:

Name:DCCH
Identity:1

Priority:0
CT Length:4
CT Value:0
TCTF Length:0
TCTF Value:0
UE ID Type:Not used
UE ID:0

Item Number 1:

Logical Channel:

Name:DCCH
Identity:2

Priority:0
CT Length:4
CT Value:1
TCTF Length:0
TCTF Value:0
UE ID Type:Not used
UE ID:0

Item Number 2:

Logical Channel:

Name:DCCH
Identity:3

Priority:0
CT Length:4
CT Value:2
TCTF Length:0
TCTF Value:0
UE ID Type:Not used
UE ID:0

Item Number 3:

Logical Channel:

Name:DCCH
Identity:4

Priority:0
CT Length:4
CT Value:3
TCTF Length:0
TCTF Value:0
UE ID Type:Not used
UE ID:0

Active Flag:1

Transport Format Combination Set:

Number Of Transport Format Combinations:2

Transport Format Combinations 0:

Transport Format:0

Transport Format Combinations 1:

Transport Format:1

#### CMAC Configuration CNF

MAC LLA @ 00:01:31.870

BTS unit: 1:1
Channel No: 0 Name: U_DPCH
CFN: 236

Message Details:

#### CMAC_Config_CNF

LLA RRC @ 00:01:31.880

Channel ID: UL-DPCH#1
Cell ID: -1

Message Details:

CMAC_Config_CNF:

cellId:-1

routingInfo:

physicalChannelIdentity:20

#### CRLC_Config_REQ

RRC LLA @ 00:01:31.880

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:1

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode)

dl_UM_RLC_Mode:

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):136

dl_RLCModeInfo: (UL_RLC_Mode)

ul_UM_RLC_Mode:

transmissionRLC_Discard:

timerBasedNoExplicit (NoExplicitDiscard):dt100

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity):1
dLlogicalChannelIdentity (LogicalChannelIdentity):1
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC UM Channel Establish REQ

LLA RLC @ 00:01:31.910

BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 240

Message Details:

Configuration Parameters:

PU Size In Bits:136

#### CRLC UM Channel Establish CNF

RLC LLA @ 00:01:31.910

BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 240

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:01:31.930

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:1

#### CRLC_Config_REQ

RRC LLA @ 00:01:31.930

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:2

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode)

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):128

dl_RLCModeInfo: (UL_RLC_Mode)

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity):2
dLlogicalChannelIdentity (LogicalChannelIdentity):2
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC AM Channel Establish REQ

LLA RLC @ 00:01:32.070

BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 0

Message Details:

Configuration Parameters:

PU Size In Bits:128

Timer Parameters:

Poll (ms):200
Poll Prohibit (ms):0
EPC (ms):0
Discard (ms):0
Poll Periodic (ms):0
Status Prohibit (ms):0
Status Periodic (ms):0
Reset (ms):500
MRW (ms):0

Protocol Parameters:

Max Dat:15
Poll PU:0
Poll SDU:1
Poll Window:99
Max Reset:1
Tx Window Size:32
Rx Window Size:32
Max MRW:0
SDU Discard Mode:No discard

Polling Triggers:

Last PU In Buffer:On
Last PU In Retransmission Buffer:On
Poll Timer:On
Every Poll-PU PU:Off
Every Poll-SDU SDU:On
Poll-Window Percent Of Transmission Buffer:On
Timer Based:Off

Status Triggers:

Missing PU:On
Timer Based:Off
EPC Mechanism:Off

#### CRLC AM Channel Establish CNF

RLC LLA @ 00:01:32.070

BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 0

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:01:32.100

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:2

#### CRLC_Config_REQ

RRC LLA @ 00:01:32.100

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:3

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode)

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):128

dl_RLCModeInfo: (UL_RLC_Mode)

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity):3
dLlogicalChannelIdentity (LogicalChannelIdentity):3
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC AM Channel Establish REQ

LLA RLC @ 00:01:32.230

BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 16

Message Details:

Configuration Parameters:

PU Size In Bits:128

Timer Parameters:

Poll (ms):200
Poll Prohibit (ms):0
EPC (ms):0
Discard (ms):0
Poll Periodic (ms):0
Status Prohibit (ms):0
Status Periodic (ms):0
Reset (ms):500
MRW (ms):0

Protocol Parameters:

Max Dat:15
Poll PU:0
Poll SDU:1
Poll Window:99
Max Reset:1
Tx Window Size:32
Rx Window Size:32
Max MRW:0
SDU Discard Mode:No discard

Polling Triggers:

Last PU In Buffer:On
Last PU In Retransmission Buffer:On
Poll Timer:On
Every Poll-PU PU:Off
Every Poll-SDU SDU:On
Poll-Window Percent Of Transmission Buffer:On
Timer Based:Off

Status Triggers:

Missing PU:On
Timer Based:Off
EPC Mechanism:Off

#### CRLC AM Channel Establish CNF

RLC LLA @ 00:01:32.230

BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 16

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:01:32.240

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:3

#### CRLC_Config_REQ

RRC LLA @ 00:01:32.240

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:4

ratType:fdd

configMessage: (CrlcConfigReq)

setup: (RBInfo)

sS_rlc_Info:

sS_ul_RLC_Mode: (DL_RLC_Mode)

dl_AM_RLC_Mode:

inSequenceDelivery:true
receivingWindowSize:rw32

dl_RLC_StatusInfo:

timerStatusProhibit:tsp200
timerEPC: Omit
missingPDU_Indicator:true
timerStatusPeriodic: Omit

sS_dl_RLC_Mode:

dl_PayloadSize (PayloadSize):128

dl_RLCModeInfo: (UL_RLC_Mode)

ul_AM_RLC_Mode:

transmissionRLC_Discard:

noDiscard (MaxDAT):dat15

transmissionWindowSize:tw32
timerRST:tr500
max_RST (MaxRST):rst1

pollingInfo:

timerPollProhibit:tpp200
timerPoll:tp200
poll_PDU: Omit
poll_SDU:sdu1
lastTransmissionPDU_Poll:true
lastRetransmissionPDU_Poll:true
pollWindow:pw99
timerPollPeriodic: Omit

rB_LogCH_Mapping:

uLlogicalChannelIdentity (LogicalChannelIdentity):4
dLlogicalChannelIdentity (LogicalChannelIdentity):4
logicalChannelType: Omit
cn_DomainIdentity: Omit

#### CRLC AM Channel Establish REQ

LLA RLC @ 00:01:32.310

BTS unit: 1:1
Channel No: 4 Name: DCCH
CFN: 24

Message Details:

Configuration Parameters:

PU Size In Bits:128

Timer Parameters:

Poll (ms):200
Poll Prohibit (ms):0
EPC (ms):0
Discard (ms):0
Poll Periodic (ms):0
Status Prohibit (ms):0
Status Periodic (ms):0
Reset (ms):500
MRW (ms):0

Protocol Parameters:

Max Dat:15
Poll PU:0
Poll SDU:1
Poll Window:99
Max Reset:1
Tx Window Size:32
Rx Window Size:32
Max MRW:0
SDU Discard Mode:No discard

Polling Triggers:

Last PU In Buffer:On
Last PU In Retransmission Buffer:On
Poll Timer:On
Every Poll-PU PU:Off
Every Poll-SDU SDU:On
Poll-Window Percent Of Transmission Buffer:On
Timer Based:Off

Status Triggers:

Missing PU:On
Timer Based:Off
EPC Mechanism:Off

#### CRLC AM Channel Establish CNF

RLC LLA @ 00:01:32.310

BTS unit: 1:1
Channel No: 4 Name: DCCH
CFN: 24

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:01:32.320

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:4

#### CRLC_Config_REQ

RRC LLA @ 00:01:32.320

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:1

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC UM Channel Release REQ

LLA RLC @ 00:01:32.390

BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 32

Message Details:

#### CRLC UM Channel Release CNF

RLC LLA @ 00:01:32.390

BTS unit: 1:1
Channel No: 1 Name: DCCH
CFN: 32

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:01:32.430

Channel ID: Rb1
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:1

#### CRLC_Config_REQ

RRC LLA @ 00:01:32.430

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:2

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC AM Channel Release REQ

LLA RLC @ 00:01:32.520

BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 45

Message Details:

#### CRLC AM Channel Release CNF

RLC LLA @ 00:01:32.520

BTS unit: 1:1
Channel No: 2 Name: DCCH
CFN: 45

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:01:32.540

Channel ID: Rb2
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:2

#### CRLC_Config_REQ

RRC LLA @ 00:01:32.540

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:3

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC AM Channel Release REQ

LLA RLC @ 00:01:32.710

BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 64

Message Details:

#### CRLC AM Channel Release CNF

RLC LLA @ 00:01:32.710

BTS unit: 1:1
Channel No: 3 Name: DCCH
CFN: 64

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:01:32.740

Channel ID: Rb3
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:3

#### CRLC_Config_REQ

RRC LLA @ 00:01:32.740

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_REQ:

cellId:-1

routingInfo:

rB_Identity:4

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC AM Channel Release REQ

LLA RLC @ 00:01:32.870

BTS unit: 1:1
Channel No: 4 Name: DCCH
CFN: 80

Message Details:

#### CRLC AM Channel Release CNF

RLC LLA @ 00:01:32.880

BTS unit: 1:1
Channel No: 4 Name: DCCH
CFN: 81

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:01:32.880

Channel ID: Rb4
Cell ID: -1

Message Details:

CRLC_Config_CNF:

cellId:-1

routingInfo:

rB_Identity:4

#### CMAC_Config_REQ

RRC LLA @ 00:01:32.880

Channel ID: DL-DPCH#1
Cell ID: -1

Message Details:

CMAC_Config_REQ:

cellId:-1

routingInfo:

physicalChannelIdentity:26

ratType:fdd

configMessage:

release:

#### CMAC Configuration REQ

LLA MAC @ 00:01:32.900

BTS unit: 1:1
Channel No: 0 Name: D_DPCH
CFN: 83

Message Details:

Configuration Parameters:

Number Of Transport Channels:0
Active Flag:0

Transport Format Combination Set:

Number Of Transport Format Combinations:0

#### CMAC Configuration CNF

MAC LLA @ 00:01:32.900

BTS unit: 1:1
Channel No: 0 Name: D_DPCH
CFN: 83

Message Details:

#### CMAC_Config_CNF

LLA RRC @ 00:01:32.910

Channel ID: DL-DPCH#1
Cell ID: -1

Message Details:

CMAC_Config_CNF:

cellId:-1

routingInfo:

physicalChannelIdentity:26

#### CMAC_Config_REQ

RRC LLA @ 00:01:32.910

Channel ID: UL-DPCH#1
Cell ID: -1

Message Details:

CMAC_Config_REQ:

cellId:-1

routingInfo:

physicalChannelIdentity:20

ratType:fdd

configMessage:

release:

#### CMAC Configuration REQ

LLA MAC @ 00:01:32.930

BTS unit: 1:1
Channel No: 0 Name: U_DPCH
CFN: 86

Message Details:

Configuration Parameters:

Number Of Transport Channels:0
Active Flag:0

Transport Format Combination Set:

Number Of Transport Format Combinations:0

#### CMAC Configuration CNF

MAC LLA @ 00:01:32.930

BTS unit: 1:1
Channel No: 0 Name: U_DPCH
CFN: 86

Message Details:

#### CMAC_Config_CNF

LLA RRC @ 00:01:32.940

Channel ID: UL-DPCH#1
Cell ID: -1

Message Details:

CMAC_Config_CNF:

cellId:-1

routingInfo:

physicalChannelIdentity:20

#### CPHY_TrCH_Release_REQ

RRC LLA @ 00:01:32.940

Channel ID: DL-DPCH#1
Cell ID: 0

Message Details:

CPHY_TrCH_Release_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:26

trchConfigType:

dch:Normal

#### CPHY Transport Channel Release REQ

LLA PHY @ 00:01:32.960

BTS unit: 1:1
Channel No: 0 Name: D_DPCH
CFN: 89

Message Details:

#### CPHY Transport Channel Release CNF

PHY LLA @ 00:01:32.960

BTS unit: 1:1
Channel No: 0 Name: D_DPCH
CFN: 89

Message Details:

#### CPHY_TrCH_Release_CNF

LLA RRC @ 00:01:32.970

Channel ID: DL-DPCH#1
Cell ID: 0

Message Details:

CPHY_TrCH_Release_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:26

#### CPHY_TrCH_Release_REQ

RRC LLA @ 00:01:32.970

Channel ID: UL-DPCH#1
Cell ID: 0

Message Details:

CPHY_TrCH_Release_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:20

trchConfigType:

dch:Normal

#### CPHY Transport Channel Release REQ

LLA PHY @ 00:01:32.990

BTS unit: 1:1
Channel No: 0 Name: U_DPCH
CFN: 92

Message Details:

#### CPHY Transport Channel Release CNF

PHY LLA @ 00:01:32.990

BTS unit: 1:1
Channel No: 0 Name: U_DPCH
CFN: 92

Message Details:

#### CPHY_TrCH_Release_CNF

LLA RRC @ 00:01:33.010

Channel ID: UL-DPCH#1
Cell ID: 0

Message Details:

CPHY_TrCH_Release_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:20

#### CPHY_RL_Release_REQ

RRC LLA @ 00:01:33.010

Channel ID: DL-DPCH#1
Cell ID: 0

Message Details:

CPHY_RL_Release_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:26

#### CPHY Radio Link Release REQ

LLA PHY @ 00:01:33.020

BTS unit: 1:1
Channel No: 0 Name: D_DPCH
CFN: 95

Message Details:

#### CPHY Radio Link Release CNF

PHY LLA @ 00:01:33.020

BTS unit: 1:1
Channel No: 0 Name: D_DPCH
CFN: 95

Message Details:

#### CPHY_RL_Release_CNF

LLA RRC @ 00:01:33.040

Channel ID: DL-DPCH#1
Cell ID: 0

Message Details:

CPHY_RL_Release_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:26

#### CPHY_RL_Release_REQ

RRC LLA @ 00:01:33.040

Channel ID: UL-DPCH#1
Cell ID: 0

Message Details:

CPHY_RL_Release_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:20

#### CPHY Radio Link Release REQ

LLA PHY @ 00:01:33.050

BTS unit: 1:1
Channel No: 0 Name: U_DPCH
CFN: 98

Message Details:

#### CPHY Radio Link Release CNF

PHY LLA @ 00:01:33.050

BTS unit: 1:1
Channel No: 0 Name: U_DPCH
CFN: 98

Message Details:

#### CPHY_RL_Release_CNF

LLA RRC @ 00:01:33.070

Channel ID: UL-DPCH#1
Cell ID: 0

Message Details:

CPHY_RL_Release_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:20

#### CRLC_Config_REQ

RRC LLA @ 00:01:33.070

Channel ID: Rb0
Cell ID: 0

Message Details:

CRLC_Config_REQ:

cellId:0

routingInfo:

rB_Identity:0

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC UM Channel Release REQ

LLA RLC @ 00:01:33.170

BTS unit: 1:1
Channel No: 1 Name: CCCH
CFN: 110

Message Details:

#### CRLC UM Channel Release CNF

RLC LLA @ 00:01:33.170

BTS unit: 1:1
Channel No: 1 Name: CCCH
CFN: 110

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:01:33.180

Channel ID: Rb0
Cell ID: 0

Message Details:

CRLC_Config_CNF:

cellId:0

routingInfo:

rB_Identity:0

#### CMAC_Config_REQ

RRC LLA @ 00:01:33.180

Channel ID: PRACH#1
Cell ID: 0

Message Details:

CMAC_Config_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:8

ratType:fdd

configMessage:

release:

#### CMAC Configuration REQ

LLA MAC @ 00:01:33.200

BTS unit: 1:1
Channel No: 0 Name: PRACH
CFN: 113

Message Details:

Configuration Parameters:

Number Of Transport Channels:0
Active Flag:0

Transport Format Combination Set:

Number Of Transport Format Combinations:0

#### CMAC Configuration CNF

MAC LLA @ 00:01:33.200

BTS unit: 1:1
Channel No: 0 Name: PRACH
CFN: 113

Message Details:

#### CMAC_Config_CNF

LLA RRC @ 00:01:33.210

Channel ID: PRACH#1
Cell ID: 0

Message Details:

CMAC_Config_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:8

#### CPHY_TrCH_Release_REQ

RRC LLA @ 00:01:33.210

Channel ID: PRACH#1
Cell ID: 0

Message Details:

CPHY_TrCH_Release_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:8

trchConfigType:

nonDch:

#### CPHY Transport Channel Release REQ

LLA PHY @ 00:01:33.220

BTS unit: 1:1
Channel No: 0 Name: PRACH
CFN: 115

Message Details:

#### CPHY Transport Channel Release CNF

PHY LLA @ 00:01:33.220

BTS unit: 1:1
Channel No: 0 Name: PRACH
CFN: 115

Message Details:

#### CPHY_TrCH_Release_CNF

LLA RRC @ 00:01:33.240

Channel ID: PRACH#1
Cell ID: 0

Message Details:

CPHY_TrCH_Release_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:8

#### CPHY_RL_Release_REQ

RRC LLA @ 00:01:33.240

Channel ID: AICH#1
Cell ID: 0

Message Details:

CPHY_RL_Release_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:7

#### CPHY Radio Link Release REQ

LLA PHY @ 00:01:33.260

BTS unit: 1:1
Channel No: 0 Name: AICH
CFN: 119

Message Details:

#### CPHY Radio Link Release CNF

PHY LLA @ 00:01:33.260

BTS unit: 1:1
Channel No: 0 Name: AICH
CFN: 119

Message Details:

#### CPHY_RL_Release_CNF

LLA RRC @ 00:01:33.270

Channel ID: AICH#1
Cell ID: 0

Message Details:

CPHY_RL_Release_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:7

#### CPHY_RL_Release_REQ

RRC LLA @ 00:01:33.270

Channel ID: PRACH#1
Cell ID: 0

Message Details:

CPHY_RL_Release_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:8

#### CPHY Radio Link Release REQ

LLA PHY @ 00:01:33.290

BTS unit: 1:1
Channel No: 0 Name: PRACH
CFN: 122

Message Details:

#### CPHY Radio Link Release CNF

PHY LLA @ 00:01:33.290

BTS unit: 1:1
Channel No: 0 Name: PRACH
CFN: 122

Message Details:

#### CPHY_RL_Release_CNF

LLA RRC @ 00:01:33.300

Channel ID: PRACH#1
Cell ID: 0

Message Details:

CPHY_RL_Release_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:8

#### CRLC_Config_REQ

RRC LLA @ 00:01:33.300

Channel ID: RbPcch
Cell ID: 0

Message Details:

CRLC_Config_REQ:

cellId:0

routingInfo:

rB_Identity:-2

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC TM Channel Release REQ

LLA RLC @ 00:01:33.350

BTS unit: 1:1
Channel No: 0 Name: PCCH
CFN: 128

Message Details:

#### CRLC TM Channel Release CNF

RLC LLA @ 00:01:33.350

BTS unit: 1:1
Channel No: 0 Name: PCCH
CFN: 128

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:01:33.370

Channel ID: RbPcch
Cell ID: 0

Message Details:

CRLC_Config_CNF:

cellId:0

routingInfo:

rB_Identity:-2

#### CMAC_Config_REQ

RRC LLA @ 00:01:33.370

Channel ID: S-CCPCH#1
Cell ID: 0

Message Details:

CMAC_Config_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:5

ratType:fdd

configMessage:

release:

#### CMAC Configuration REQ

LLA MAC @ 00:01:33.380

BTS unit: 1:1
Channel No: 0 Name: S_CCPCH
CFN: 131

Message Details:

Configuration Parameters:

Number Of Transport Channels:0
Active Flag:0

Transport Format Combination Set:

Number Of Transport Format Combinations:0

#### CMAC Configuration CNF

MAC LLA @ 00:01:33.380

BTS unit: 1:1
Channel No: 0 Name: S_CCPCH
CFN: 131

Message Details:

#### CMAC_Config_CNF

LLA RRC @ 00:01:33.400

Channel ID: S-CCPCH#1
Cell ID: 0

Message Details:

CMAC_Config_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:5

#### CPHY_TrCH_Release_REQ

RRC LLA @ 00:01:33.400

Channel ID: S-CCPCH#1
Cell ID: 0

Message Details:

CPHY_TrCH_Release_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:5

trchConfigType:

nonDch:

#### CPHY Transport Channel Release REQ

LLA PHY @ 00:01:33.410

BTS unit: 1:1
Channel No: 0 Name: S_CCPCH
CFN: 134

Message Details:

#### CPHY Transport Channel Release CNF

PHY LLA @ 00:01:33.410

BTS unit: 1:1
Channel No: 0 Name: S_CCPCH
CFN: 134

Message Details:

#### CPHY_TrCH_Release_CNF

LLA RRC @ 00:01:33.430

Channel ID: S-CCPCH#1
Cell ID: 0

Message Details:

CPHY_TrCH_Release_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:5

#### CPHY_RL_Release_REQ

RRC LLA @ 00:01:33.430

Channel ID: PICH#1
Cell ID: 0

Message Details:

CPHY_RL_Release_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:6

#### CPHY Radio Link Release REQ

LLA PHY @ 00:01:33.440

BTS unit: 1:1
Channel No: 0 Name: PICH
CFN: 137

Message Details:

#### CPHY Radio Link Release CNF

PHY LLA @ 00:01:33.440

BTS unit: 1:1
Channel No: 0 Name: PICH
CFN: 137

Message Details:

#### CPHY_RL_Release_CNF

LLA RRC @ 00:01:33.460

Channel ID: PICH#1
Cell ID: 0

Message Details:

CPHY_RL_Release_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:6

#### CPHY_RL_Release_REQ

RRC LLA @ 00:01:33.460

Channel ID: S-CCPCH#1
Cell ID: 0

Message Details:

CPHY_RL_Release_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:5

#### CPHY Radio Link Release REQ

LLA PHY @ 00:01:33.470

BTS unit: 1:1
Channel No: 0 Name: S_CCPCH
CFN: 140

Message Details:

#### CPHY Radio Link Release CNF

PHY LLA @ 00:01:33.470

BTS unit: 1:1
Channel No: 0 Name: S_CCPCH
CFN: 140

Message Details:

#### CPHY_RL_Release_CNF

LLA RRC @ 00:01:33.490

Channel ID: S-CCPCH#1
Cell ID: 0

Message Details:

CPHY_RL_Release_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:5

#### CRLC_Config_REQ

RRC LLA @ 00:01:33.490

Channel ID: RbBcch
Cell ID: 0

Message Details:

CRLC_Config_REQ:

cellId:0

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC TM Channel Release REQ

LLA RLC @ 00:01:33.510

BTS unit: 1:1
Channel No: 0 Name: BCCH
CFN: 144

Message Details:

#### CRLC TM Channel Release CNF

RLC LLA @ 00:01:33.510

BTS unit: 1:1
Channel No: 0 Name: BCCH
CFN: 144

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:01:33.520

Channel ID: RbBcch
Cell ID: 0

Message Details:

CRLC_Config_CNF:

cellId:0

routingInfo:

rB_Identity:-1

#### CMAC_Config_REQ

RRC LLA @ 00:01:33.520

Channel ID: P-CCPCH
Cell ID: 0

Message Details:

CMAC_Config_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:4

ratType:fdd

configMessage:

release:

#### CMAC Configuration REQ

LLA MAC @ 00:01:33.540

BTS unit: 1:1
Channel No: 0 Name: P_CCPCH
CFN: 147

Message Details:

Configuration Parameters:

Number Of Transport Channels:0
Active Flag:0

Transport Format Combination Set:

Number Of Transport Format Combinations:0

#### CMAC Configuration CNF

MAC LLA @ 00:01:33.540

BTS unit: 1:1
Channel No: 0 Name: P_CCPCH
CFN: 147

Message Details:

#### CMAC_Config_CNF

LLA RRC @ 00:01:33.550

Channel ID: P-CCPCH
Cell ID: 0

Message Details:

CMAC_Config_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:4

#### CPHY_TrCH_Release_REQ

RRC LLA @ 00:01:33.550

Channel ID: P-CCPCH
Cell ID: 0

Message Details:

CPHY_TrCH_Release_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:4

trchConfigType:

nonDch:

#### CPHY Transport Channel Release REQ

LLA PHY @ 00:01:33.570

BTS unit: 1:1
Channel No: 0 Name: P_CCPCH
CFN: 150

Message Details:

#### CPHY Transport Channel Release CNF

PHY LLA @ 00:01:33.570

BTS unit: 1:1
Channel No: 0 Name: P_CCPCH
CFN: 150

Message Details:

#### CPHY_TrCH_Release_CNF

LLA RRC @ 00:01:33.580

Channel ID: P-CCPCH
Cell ID: 0

Message Details:

CPHY_TrCH_Release_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:4

#### CPHY_RL_Release_REQ

RRC LLA @ 00:01:33.580

Channel ID: S-SCH
Cell ID: 0

Message Details:

CPHY_RL_Release_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:2

#### CPHY Radio Link Release REQ

LLA PHY @ 00:01:33.600

BTS unit: 1:1
Channel No: 0 Name: S_SCH
CFN: 153

Message Details:

#### CPHY Radio Link Release CNF

PHY LLA @ 00:01:33.600

BTS unit: 1:1
Channel No: 0 Name: S_SCH
CFN: 153

Message Details:

#### CPHY_RL_Release_CNF

LLA RRC @ 00:01:33.620

Channel ID: S-SCH
Cell ID: 0

Message Details:

CPHY_RL_Release_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:2

#### CPHY_RL_Release_REQ

RRC LLA @ 00:01:33.620

Channel ID: P-SCH
Cell ID: 0

Message Details:

CPHY_RL_Release_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:1

#### CPHY Radio Link Release REQ

LLA PHY @ 00:01:33.630

BTS unit: 1:1
Channel No: 0 Name: P_SCH
CFN: 156

Message Details:

#### CPHY Radio Link Release CNF

PHY LLA @ 00:01:33.630

BTS unit: 1:1
Channel No: 0 Name: P_SCH
CFN: 156

Message Details:

#### CPHY_RL_Release_CNF

LLA RRC @ 00:01:33.650

Channel ID: P-SCH
Cell ID: 0

Message Details:

CPHY_RL_Release_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:1

#### CPHY_RL_Release_REQ

RRC LLA @ 00:01:33.650

Channel ID: P-CCPCH
Cell ID: 0

Message Details:

CPHY_RL_Release_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:4

#### CPHY Radio Link Release REQ

LLA PHY @ 00:01:33.660

BTS unit: 1:1
Channel No: 0 Name: P_CCPCH
CFN: 159

Message Details:

#### CPHY Radio Link Release CNF

PHY LLA @ 00:01:33.660

BTS unit: 1:1
Channel No: 0 Name: P_CCPCH
CFN: 159

Message Details:

#### CPHY_RL_Release_CNF

LLA RRC @ 00:01:33.680

Channel ID: P-CCPCH
Cell ID: 0

Message Details:

CPHY_RL_Release_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:4

#### CPHY_RL_Release_REQ

RRC LLA @ 00:01:33.680

Channel ID: P-CPICH
Cell ID: 0

Message Details:

CPHY_RL_Release_REQ:

cellId:0

routingInfo:

physicalChannelIdentity:0

#### CPHY Radio Link Release REQ

LLA PHY @ 00:01:33.690

BTS unit: 1:1
Channel No: 0 Name: P_CPICH
CFN: 162

Message Details:

#### CPHY Radio Link Release CNF

PHY LLA @ 00:01:33.690

BTS unit: 1:1
Channel No: 0 Name: P_CPICH
CFN: 162

Message Details:

#### CPHY_RL_Release_CNF

LLA RRC @ 00:01:33.710

Channel ID: P-CPICH
Cell ID: 0

Message Details:

CPHY_RL_Release_CNF:

cellId:0

routingInfo:

physicalChannelIdentity:0

#### CRLC_Config_REQ

RRC LLA @ 00:01:33.710

Channel ID: Rb0
Cell ID: 3

Message Details:

CRLC_Config_REQ:

cellId:3

routingInfo:

rB_Identity:0

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC UM Channel Release REQ

LLA RLC @ 00:01:33.820

BTS unit: 1:2
Channel No: 1 Name: CCCH
CFN: 175

Message Details:

#### CRLC UM Channel Release CNF

RLC LLA @ 00:01:33.820

BTS unit: 1:2
Channel No: 1 Name: CCCH
CFN: 175

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:01:33.850

Channel ID: Rb0
Cell ID: 3

Message Details:

CRLC_Config_CNF:

cellId:3

routingInfo:

rB_Identity:0

#### CMAC_Config_REQ

RRC LLA @ 00:01:33.850

Channel ID: PRACH#1
Cell ID: 3

Message Details:

CMAC_Config_REQ:

cellId:3

routingInfo:

physicalChannelIdentity:8

ratType:fdd

configMessage:

release:

#### CMAC Configuration REQ

LLA MAC @ 00:01:33.870

BTS unit: 1:2
Channel No: 0 Name: PRACH
CFN: 180

Message Details:

Configuration Parameters:

Number Of Transport Channels:0
Active Flag:0

Transport Format Combination Set:

Number Of Transport Format Combinations:0

#### CMAC Configuration CNF

MAC LLA @ 00:01:33.870

BTS unit: 1:2
Channel No: 0 Name: PRACH
CFN: 180

Message Details:

#### CMAC_Config_CNF

LLA RRC @ 00:01:33.880

Channel ID: PRACH#1
Cell ID: 3

Message Details:

CMAC_Config_CNF:

cellId:3

routingInfo:

physicalChannelIdentity:8

#### CPHY_TrCH_Release_REQ

RRC LLA @ 00:01:33.880

Channel ID: PRACH#1
Cell ID: 3

Message Details:

CPHY_TrCH_Release_REQ:

cellId:3

routingInfo:

physicalChannelIdentity:8

trchConfigType:

nonDch:

#### CPHY Transport Channel Release REQ

LLA PHY @ 00:01:33.900

BTS unit: 1:2
Channel No: 0 Name: PRACH
CFN: 183

Message Details:

#### CPHY Transport Channel Release CNF

PHY LLA @ 00:01:33.900

BTS unit: 1:2
Channel No: 0 Name: PRACH
CFN: 183

Message Details:

#### CPHY_TrCH_Release_CNF

LLA RRC @ 00:01:33.910

Channel ID: PRACH#1
Cell ID: 3

Message Details:

CPHY_TrCH_Release_CNF:

cellId:3

routingInfo:

physicalChannelIdentity:8

#### CPHY_RL_Release_REQ

RRC LLA @ 00:01:33.910

Channel ID: AICH#1
Cell ID: 3

Message Details:

CPHY_RL_Release_REQ:

cellId:3

routingInfo:

physicalChannelIdentity:7

#### CPHY Radio Link Release REQ

LLA PHY @ 00:01:33.930

BTS unit: 1:2
Channel No: 0 Name: AICH
CFN: 186

Message Details:

#### CPHY Radio Link Release CNF

PHY LLA @ 00:01:33.930

BTS unit: 1:2
Channel No: 0 Name: AICH
CFN: 186

Message Details:

#### CPHY_RL_Release_CNF

LLA RRC @ 00:01:33.940

Channel ID: AICH#1
Cell ID: 3

Message Details:

CPHY_RL_Release_CNF:

cellId:3

routingInfo:

physicalChannelIdentity:7

#### CPHY_RL_Release_REQ

RRC LLA @ 00:01:33.940

Channel ID: PRACH#1
Cell ID: 3

Message Details:

CPHY_RL_Release_REQ:

cellId:3

routingInfo:

physicalChannelIdentity:8

#### CPHY Radio Link Release REQ

LLA PHY @ 00:01:33.960

BTS unit: 1:2
Channel No: 0 Name: PRACH
CFN: 189

Message Details:

#### CPHY Radio Link Release CNF

PHY LLA @ 00:01:33.960

BTS unit: 1:2
Channel No: 0 Name: PRACH
CFN: 189

Message Details:

#### CPHY_RL_Release_CNF

LLA RRC @ 00:01:33.970

Channel ID: PRACH#1
Cell ID: 3

Message Details:

CPHY_RL_Release_CNF:

cellId:3

routingInfo:

physicalChannelIdentity:8

#### CRLC_Config_REQ

RRC LLA @ 00:01:33.970

Channel ID: RbPcch
Cell ID: 3

Message Details:

CRLC_Config_REQ:

cellId:3

routingInfo:

rB_Identity:-2

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC TM Channel Release REQ

LLA RLC @ 00:01:33.990

BTS unit: 1:2
Channel No: 0 Name: PCCH
CFN: 192

Message Details:

#### CRLC TM Channel Release CNF

RLC LLA @ 00:01:33.990

BTS unit: 1:2
Channel No: 0 Name: PCCH
CFN: 192

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:01:34.010

Channel ID: RbPcch
Cell ID: 3

Message Details:

CRLC_Config_CNF:

cellId:3

routingInfo:

rB_Identity:-2

#### CMAC_Config_REQ

RRC LLA @ 00:01:34.010

Channel ID: S-CCPCH#1
Cell ID: 3

Message Details:

CMAC_Config_REQ:

cellId:3

routingInfo:

physicalChannelIdentity:5

ratType:fdd

configMessage:

release:

#### CMAC_Config_CNF

LLA RRC @ 00:01:34.020

Channel ID: S-CCPCH#1
Cell ID: 3

Message Details:

CMAC_Config_CNF:

cellId:3

routingInfo:

physicalChannelIdentity:5

#### CPHY_TrCH_Release_REQ

RRC LLA @ 00:01:34.020

Channel ID: S-CCPCH#1
Cell ID: 3

Message Details:

CPHY_TrCH_Release_REQ:

cellId:3

routingInfo:

physicalChannelIdentity:5

trchConfigType:

nonDch:

#### CPHY Transport Channel Release REQ

LLA PHY @ 00:01:34.040

BTS unit: 1:2
Channel No: 0 Name: S_CCPCH
CFN: 197

Message Details:

#### CPHY Transport Channel Release CNF

PHY LLA @ 00:01:34.040

BTS unit: 1:2
Channel No: 0 Name: S_CCPCH
CFN: 197

Message Details:

#### CPHY_TrCH_Release_CNF

LLA RRC @ 00:01:34.050

Channel ID: S-CCPCH#1
Cell ID: 3

Message Details:

CPHY_TrCH_Release_CNF:

cellId:3

routingInfo:

physicalChannelIdentity:5

#### CPHY_RL_Release_REQ

RRC LLA @ 00:01:34.050

Channel ID: PICH#1
Cell ID: 3

Message Details:

CPHY_RL_Release_REQ:

cellId:3

routingInfo:

physicalChannelIdentity:6

#### CPHY Radio Link Release REQ

LLA PHY @ 00:01:34.070

BTS unit: 1:2
Channel No: 0 Name: PICH
CFN: 200

Message Details:

#### CPHY Radio Link Release CNF

PHY LLA @ 00:01:34.070

BTS unit: 1:2
Channel No: 0 Name: PICH
CFN: 200

Message Details:

#### CPHY_RL_Release_CNF

LLA RRC @ 00:01:34.080

Channel ID: PICH#1
Cell ID: 3

Message Details:

CPHY_RL_Release_CNF:

cellId:3

routingInfo:

physicalChannelIdentity:6

#### CPHY_RL_Release_REQ

RRC LLA @ 00:01:34.080

Channel ID: S-CCPCH#1
Cell ID: 3

Message Details:

CPHY_RL_Release_REQ:

cellId:3

routingInfo:

physicalChannelIdentity:5

#### CPHY Radio Link Release REQ

LLA PHY @ 00:01:34.100

BTS unit: 1:2
Channel No: 0 Name: S_CCPCH
CFN: 203

Message Details:

#### CPHY Radio Link Release CNF

PHY LLA @ 00:01:34.100

BTS unit: 1:2
Channel No: 0 Name: S_CCPCH
CFN: 203

Message Details:

#### CPHY_RL_Release_CNF

LLA RRC @ 00:01:34.120

Channel ID: S-CCPCH#1
Cell ID: 3

Message Details:

CPHY_RL_Release_CNF:

cellId:3

routingInfo:

physicalChannelIdentity:5

#### CRLC_Config_REQ

RRC LLA @ 00:01:34.120

Channel ID: RbBcch
Cell ID: 3

Message Details:

CRLC_Config_REQ:

cellId:3

routingInfo:

rB_Identity:-1

ratType:fdd

configMessage: (CrlcConfigReq)

release:

#### CRLC TM Channel Release REQ

LLA RLC @ 00:01:34.150

BTS unit: 1:2
Channel No: 0 Name: BCCH
CFN: 208

Message Details:

#### CRLC TM Channel Release CNF

RLC LLA @ 00:01:34.150

BTS unit: 1:2
Channel No: 0 Name: BCCH
CFN: 208

Message Details:

#### CRLC_Config_CNF

LLA RRC @ 00:01:34.160

Channel ID: RbBcch
Cell ID: 3

Message Details:

CRLC_Config_CNF:

cellId:3

routingInfo:

rB_Identity:-1

#### CMAC_Config_REQ

RRC LLA @ 00:01:34.160

Channel ID: P-CCPCH
Cell ID: 3

Message Details:

CMAC_Config_REQ:

cellId:3

routingInfo:

physicalChannelIdentity:4

ratType:fdd

configMessage:

release:

#### CMAC Configuration REQ

LLA MAC @ 00:01:34.180

BTS unit: 1:2
Channel No: 0 Name: P_CCPCH
CFN: 211

Message Details:

Configuration Parameters:

Number Of Transport Channels:0
Active Flag:0

Transport Format Combination Set:

Number Of Transport Format Combinations:0

#### CMAC Configuration CNF

MAC LLA @ 00:01:34.180

BTS unit: 1:2
Channel No: 0 Name: P_CCPCH
CFN: 211

Message Details:

#### CMAC_Config_CNF

LLA RRC @ 00:01:34.190

Channel ID: P-CCPCH
Cell ID: 3

Message Details:

CMAC_Config_CNF:

cellId:3

routingInfo:

physicalChannelIdentity:4

#### CPHY_TrCH_Release_REQ

RRC LLA @ 00:01:34.190

Channel ID: P-CCPCH
Cell ID: 3

Message Details:

CPHY_TrCH_Release_REQ:

cellId:3

routingInfo:

physicalChannelIdentity:4

trchConfigType:

nonDch:

#### CPHY Transport Channel Release REQ

LLA PHY @ 00:01:34.210

BTS unit: 1:2
Channel No: 0 Name: P_CCPCH
CFN: 214

Message Details:

#### CPHY Transport Channel Release CNF

PHY LLA @ 00:01:34.210

BTS unit: 1:2
Channel No: 0 Name: P_CCPCH
CFN: 214

Message Details:

#### CPHY_TrCH_Release_CNF

LLA RRC @ 00:01:34.220

Channel ID: P-CCPCH
Cell ID: 3

Message Details:

CPHY_TrCH_Release_CNF:

cellId:3

routingInfo:

physicalChannelIdentity:4

#### CPHY_RL_Release_REQ

RRC LLA @ 00:01:34.220

Channel ID: S-SCH
Cell ID: 3

Message Details:

CPHY_RL_Release_REQ:

cellId:3

routingInfo:

physicalChannelIdentity:2

#### CPHY Radio Link Release REQ

LLA PHY @ 00:01:34.240

BTS unit: 1:2
Channel No: 0 Name: S_SCH
CFN: 217

Message Details:

#### CPHY Radio Link Release CNF

PHY LLA @ 00:01:34.240

BTS unit: 1:2
Channel No: 0 Name: S_SCH
CFN: 217

Message Details:

#### CPHY_RL_Release_CNF

LLA RRC @ 00:01:34.260

Channel ID: S-SCH
Cell ID: 3

Message Details:

CPHY_RL_Release_CNF:

cellId:3

routingInfo:

physicalChannelIdentity:2

#### CPHY_RL_Release_REQ

RRC LLA @ 00:01:34.260

Channel ID: P-SCH
Cell ID: 3

Message Details:

CPHY_RL_Release_REQ:

cellId:3

routingInfo:

physicalChannelIdentity:1

#### CPHY Radio Link Release REQ

LLA PHY @ 00:01:34.270

BTS unit: 1:2
Channel No: 0 Name: P_SCH
CFN: 220

Message Details:

#### CPHY Radio Link Release CNF

PHY LLA @ 00:01:34.270

BTS unit: 1:2
Channel No: 0 Name: P_SCH
CFN: 220

Message Details:

#### CPHY_RL_Release_CNF

LLA RRC @ 00:01:34.290

Channel ID: P-SCH
Cell ID: 3

Message Details:

CPHY_RL_Release_CNF:

cellId:3

routingInfo:

physicalChannelIdentity:1

#### CPHY_RL_Release_REQ

RRC LLA @ 00:01:34.290

Channel ID: P-CCPCH
Cell ID: 3

Message Details:

CPHY_RL_Release_REQ:

cellId:3

routingInfo:

physicalChannelIdentity:4

#### CPHY Radio Link Release REQ

LLA PHY @ 00:01:34.300

BTS unit: 1:2
Channel No: 0 Name: P_CCPCH
CFN: 223

Message Details:

#### CPHY Radio Link Release CNF

PHY LLA @ 00:01:34.300

BTS unit: 1:2
Channel No: 0 Name: P_CCPCH
CFN: 223

Message Details:

#### CPHY_RL_Release_CNF

LLA RRC @ 00:01:34.320

Channel ID: P-CCPCH
Cell ID: 3

Message Details:

CPHY_RL_Release_CNF:

cellId:3

routingInfo:

physicalChannelIdentity:4

#### CPHY_RL_Release_REQ

RRC LLA @ 00:01:34.320

Channel ID: P-CPICH
Cell ID: 3

Message Details:

CPHY_RL_Release_REQ:

cellId:3

routingInfo:

physicalChannelIdentity:0

#### CPHY Radio Link Release REQ

LLA PHY @ 00:01:34.330

BTS unit: 1:2
Channel No: 0 Name: P_CPICH
CFN: 226

Message Details:

#### CPHY Radio Link Release CNF

PHY LLA @ 00:01:34.330

BTS unit: 1:2
Channel No: 0 Name: P_CPICH
CFN: 226

Message Details:

#### CPHY_RL_Release_CNF

LLA RRC @ 00:01:34.350

Channel ID: P-CPICH
Cell ID: 3

Message Details:

CPHY_RL_Release_CNF:

cellId:3

routingInfo:

physicalChannelIdentity:0

#### CGEN Stop REQ

RRC PHY @ 00:01:35.400

Message Details:

#### CGEN Stop CNF

PHY RRC @ 00:01:35.400

Message Details: