3GPP TSG-T2 #7 / ETSI SMG4
Ystad, SWEDEN, 22-26 November 1999	TSGT2#7(99)967	

Agenda Item:	

Source:	CETECOM

Title:	Comment to TS 101 369 V7.0.0

Document for:	Action

___________________________________________________________________________

-----Original Message-----
From: Heinz Christoph, Essen [mailto:Christoph.Heinz@cetecom.de]
Sent: 19 November 1999 10:17
To: Editor
Subject: comment to TS 101 369 V7.0.0

Dear Sirs,

at 5.2.1.5 Length indicator in the sentence before figure 4 inside the
brackets,
it must be stated "(only present when the EA field in the first byte is set
to 0)".
EA=1 means no second octet, because the first one is the last.

Best Regards,

Christoph Heinz
Cetecom GmbH
Germany
Project Development
Tel.:	          +49 2054 9519-957
Fax:	          +49 2054 9519-21
Mobile:	          +49 172 208 3953
e-mail:	          mailto:christoph.heinz@cetecom.de