3GPP TSG-RAN WG2 #110-e TDoc R2-200xxxx

**Electronic, June 1st – June 12th, 2020**

Agenda Item: 6.4.2.2

Source: ZTE Corporation, Sanechips

Title: Summary of NR V2X UE cell (re-)selection related contribution

Document for: Discussion, Decision

# Introduction

In this contribution, we will give a summarize of all contributions related to NR V2X cell selection/ reselection, which is based on the following contributions.

|  |  |  |
| --- | --- | --- |
| TDoc No. | Title | Source |
| R2-2002829 | Discussion on inter-RAT Cell Selection/Reselection | CATT |
| R2-2003097 | Remaining issues of cell (re)selection for NR V2X | Lenovo, Motorola Mobility |
| R2-2003515 | Remaining issues on cell reselection for sidelink in TS 38.304 | Huawei, HiSilicon |
| R2-2003721 | Finalising cell reselection for V2X | Samsung |

In details, all proposals raised in those contributions are quite essential at this stage. Thus, all issues listed out in the following are marked with essential.

# Discussion

## [Essential] Rel-16 V2X UE performing cell (re-)selection in RRC connected state

According to the description in [1], it clarifies that in LTE sidelink and V2X, UE is allowed to perform cell selection/reselection under RRC connected mode. The reason is that the SL/V2X UE may also work as a normal Uu UE, then it may access into RRC connected mode due to Uu services, but the eNB which it accesses into may not support SL/V2X SL features. As the consequence, the UE may still need to choose another cell for SL configurations if it has the SL traffic. Thus, in their opinion, the same principle should be applied to NR V2X as well. Thus,

**Question 1: Whether the procedure of cell selection and reselection should apply to RRC\_CONNECTED UE as well ?**

**- Alt 1: Yes**

**- Alt 2: No**

|  |  |  |
| --- | --- | --- |
| **Company** | **Option** | **Comments (if any)** |
| Ericsson | Yes | Ok to follow LTE principle. |
| vivo | Yes for cell selection, FFS for cell reselection  | The section of ‘11.4 Cell selection and reselection for sidelink’, saying that ‘the requirements defined in this clause for sidelink operation apply for UEs in RRC\_IDLE and in RRC\_CONNECTED’ was captured and agreed in the CR in RAN2 #88, but after tracking some of the discussions then we have some kind of feeling that the reason could just be that the UE shall perform cell selection during RRC re-establishment when the UE is in CONNECTED, rather than from the service point of view. For cell reselection, it seems that the scenario for RRC\_CONNECTED UE to perform cell reselection based on sidelink service was not really discussed then, and in fact this may have impact on the whole RRM design (e.g. the UE may reselect to another cell without NW handover command and awareness), so we need to be careful about this. |
| CATT | Yes | Same as LTE  |
| Huawei | Yes | Follow LTE SL (TS 36.304, subclause 11.4) |
| ZTE | Yes | We should follow LTE SL |

## [Essential] On-demand SI providing anchor carrier configuration

In LTE, SIBs will only be configured to the camping UE via broadcast communication. Thus, the UE can recognize whether the cell can provide sidelink configuration or only anchor carrier configuration via reading the related SIB message. However, when it comes to NR V2X, the SIB is allowed to be configured to the UE not only via broadcast, but also can be through on-demand SI. If the V2X SIB is configured to the UE through on-demand SI, the UE cannot recognize whether there is detailed V2X configuration or only anchor carrier configuration until it performing random access and acquire the on-demand SI, where it is somehow a waste of time. Therefore, to avoid this issue, the following alternatives are proposed, as concluded in [2],[3] and [4]:

Alt 1: If a cell providing only anchor carrier configuration, the cell should always broadcast the V2X SIB.

Alt 2: If the NR V2X SI is provided on-demand, then the UE does not prioritize this cell.

Alt 3: If a carrier doesn’t broadcast the V2X SIB but provide it by on-demand, then this frequency should be indicated by other frequency as anchor frequency in the V2X SIB.

Alt 4: Introduce an IE in SIB 1,2/4 to indicate whether the cell will only providing anchor carrier configuration.

**Question 2: Targeting on the issue that cell broadcasting only anchor carrier configuration via on demand SI, which one of the following solutions shall be adopted ?**

**- Alt 1: If a cell providing only anchor carrier configuration, it should always broadcast the V2X SIB.**

**- Alt 2: If the NR V2X SI is provided on-demand, then the UE does not prioritize this cell.**

**- Alt 3:If a carrier doesn’t broadcast the V2X SIB but provide it by on-demand, then this frequency should be indicated by other frequency as anchor frequency in the V2X SIB.**

**- Alt 4:Introduce an IE in SIB 1,2/4 to indicate whether the cell will only providing anchor carrier configuration.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Option** | **Comments (if any)** |
| Ericsson | Alt 3 and upon implementation | In our view, this issue can be handled by NW implementation, i.e. this frequency might be indicated by other frequency as anchor frequency in V2X SIB. We don’t see specification impact.  |
| vivo | Alt 1 | This is already discussed in previous meeting’s offline discussion(R2-2001974), and we think alt-1 is the simplest way to solve this problem by network implementation. |
| CATT | Alt 4, in SIB 1 | **Introduce an IE in SIB 1 to indicate whether the cell will only providing anchor carrier configuration.**For Alt1 and Alt2, since the V2X SI is broadcasted or on demand is up to gNB implementation. Alt1 explicitly restricts gNB can’t provide only anchor carrier configuration by on demand. For Alt2, the UE doesn’t distinguish the V2X configuration in the SIB12 is anchor carrier configuration or not. The V2X capable UE may camp on the cell without V2X configuration when Alt2 is agreed. To avoid this issue, gNB should either provide SIB12 by broadcast or indicates the cell information in which provides V2X configuration in every cell. It will not provision in specification. For Alt3, it can be only used for cell reselection. However, for cell selection, the UE may camp on the cell only provides anchor carrier configuration first, and then reselect to the cell provides SL configuration. To avoid UE (re)selects to the cell only provides anchor carrier configuration, an IE in SIB 1 should be introduced to indicate whether the cell will only providing anchor carrier configuration..  |
| Huawei | Alt 4. | In Alt 4, [SIB 1,2/4] may be an editorial mistake, it should be [SIB 1,3/4]?Alt 1 has restriction on network implementation, which is not a good solution from the network vendors’ perspective. A key reason why there is no agreement on this issue in the RAN2#109 meeting is that some companies object the restriction on network implementation.Alt 2 means that even for the cells providing V2X SL configurations, if the V2X SI is provided on-demand, then the UE does not prioritize these cells, which is not reasonable according to the related agreements. To be specific, when the UE cannot find any cell always broadcasting V2X SL configurations while some neighboring cells provide V2X SL configuration on-demand, it is possible for the UE to reselect a cell providing only anchor carrier configuration (i.e. without V2X SL configuration).Alt 3 is to restrict the network to put all the neighbouring frequencies that providing V2X SL configurations into “AnchorCarrierFreqList”, so that all the neighboring frequencies which provide V2X SIB but are not within “AnchorCarrierFreqList” can be considered only providing anchor carrier configuration. However, as in Alt1, the restrictions on network implementation is not a good solution. Moreover, in Alt 3 “a carrier that doesn’t broadcast the V2X SIB but provide it by on-demand” may only provide anchor carrier configuration, which is not align with the definition of as follows.***sl-NR-AnchorCarrierFreqList***This field indicates the NR anchor carrier frequency list, which can provide the NR sidelink communication configurations. |
| ZTE | Alt 3  | Alt 3 is a network implementation method which can solve thisissue without too much specification effort, but as Huawei mentioned, alt 3 may need to modify the definition of sl-NR-AnchorCarrierFreqList, |

## [Essential] How to use pre-configuration[4][5]

Currently, there are three types of sidelink carrier:

-Type 1:Frequency which can provide both NR sidelink communication configuration and LTE sidelink communication configuration.

-Type 2:Frequency which can provide either NR sidelink communication configuration and LTE sidelink communication configuration.

-Type 3: Frequency which cannot provide any sidelink communication configuration.

If there are only type 2 frequencies. Specifically, if some type 2 frequencies can provide only NR SL configuration, the other type 2 frequencies can provide only LTE SL configuration. On the other hand, the UE can support both NR and LTE SL traffics. When the UE camping on any type 2 frequencies, it can only acquire SL configuration for one SL RAT, but actually the UE may be in coverage for both of the two SL RATs since UE will determine its coverage status of each SL RAT independently as per current specification. Then for the other SL RAT of which UE cannot acquire SL configuration from the camping cell, whther pre-configuration is allowed to be used ?

**Question 3: For the case that if UE supports both NR and LTE SL, but UE’s camped cell can only provide one SL RAT configuration, whether pre-configured SL resource can be used on the other RAT if the UE is also in-coverage of that RAT ?**

**- Alt 1: Yes**

**- Alt 2: No**

|  |  |  |
| --- | --- | --- |
| **Company** | **Option** | **Comments (if any)** |
| Ericsson | No | When it is LTE V2X operating in unlicensed spectrum, it is fine. However, if a NR V2X UE using licensed spectrum within a cell according to pre-configuration and not known by the cell, it might cause problems in terms of resource allocation for other traffics within the cell. Better to avoid it overall.  |
| vivo | Yes | This is also discussed before and we think pre-configuration can work in this case. No big issue seems to be identified here. The cell is supposed to be able to know the resources configured in pre-configuration. |
| CATT | No | It may introduce interference between the UEs using pre-configuration and other UEs using network configuration, especially the interference to the dedicated grant configured by gNB. |
| Huawei | No need to discuss | No need to discuss this issue. Whether the UE uses preconfiguration on a SL RAT should depend on the V2X sidelink communication transmission procedure in TS 36.331 and NR sidelink communication transmission procedure in TS 38.331, respectively. If the UE on an SL RAT meets the condition for using preconfiguration, the UE uses it; otherwise, it does not. What’s the extra problem?The key point here is that the transmission/reception procedure for NR SL and that for V2X SL are independent, so how the resource (pre)configuration for one SL RAT is used shouldn’t be coupled with the other SL RAT. |
| ZTE | No need to discuss | Share the same view with Huawei, not only the determination of UE’s coverage status for each RAT is independent, but also the transmission/reception procedure for each RAT is also independent.  |

Moreover, if pre-configuration is not allowed to use in the above mentioned case, then several alternatives to help UE acquire V2X configuration are provided in [4],[5].

* Option 1: UE performs cell reselection to select the carrier which provides the SL configuration of the other RAT.
* Option 2: UE requests the SL configuration of the other RAT from the camped cell.
* Option 3: UE a quires the SL configuration of the other RAT by reading the broadcast V2X SIB on the concerned carrier.

Then RAN2 should filter out one workable solution to help UE acquire V2X related configuration.

**Question 4: If pre-configuration is not allowed for the UE to use which is in coverage, then which one of the following solution shall be adopted ?**

**- Alt 1: UE performs cell reselection to select the carrier which provides the SL configuration of the other RAT.**

**- Alt 2: UE requests the SL configuration of the other RAT from the camped cell.**

**- Alt 3: UE acquires the SL configuration of the other RAT by reading the broadcast V2X SIB on the concerned carrier.**

**- Alt 4: Others (Please specify)**

|  |  |  |
| --- | --- | --- |
| **Company** | **Option** | **Comments (if any)** |
| Ericsson | Option 1 | we don’t need to optimize the scenario.  |
| vivo | Alt 3 with comments | As comments in Question 3, we think the pre-configuration can work in this case. But if majority think there is a big issue to use pre-configuration and alternatives are needed, then we prefer to go for alt-3, which seems aligned with LTE solution to some extent, because in LTE the UE seems also capable to read the broadcast V2X SIB on the concerned carrier which is not serving frequency for transmission and reception. |
| CATT | Alt 1 for on-demand SIAlt 3 for broadcast SI | If the V2X SIB is by on-demand, UE only can perform cell reselection to select the carrier to acquire the SL configuration of the other RAT.If the V2X SIB is by broadcast, UE can acquire the SL configuration of the other RAT by reading the broadcast V2X SIB‎, which follows the LTE rule. |
| Huawei | No need to discuss | Same comments as to Q3. |
| ZTE | No need to discuss | Same comments as Q3. |

# Conclusion

In this contribution, we have summarized all principle opinions from NR V2X cell selection/reselection contributions, a brunch of proposals have been provided in the following:

# References

1. R2-2003515 Remaining issues on cell reselection for sidelink in TS 38.304 Huawei, HiSilicon
2. R2-2001974 Report of offline discussion 709 ZTE Corporation, Sanechips
3. R2-2003097 Remaining issues of cell (re)selection for NR V2X Lenovo, Motorola Mobility
4. R2-2002829 Discussion on inter-RAT Cell Selection/Reselection CATT
5. R2-2003721 Finalising cell reselection for V2X Samsung