**3GPP TSG- Meeting #**

**,**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.1* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  |  | **CR** |  | **rev** |  | **Current version:** |  |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network | **X** | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Update on V2X UE capability | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | OPPO | | | | | | | | | |
| ***Source to TSG:*** | RAN2 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | 5G\_V2X\_NRSL-Core | | | | |  | ***Date:*** | | | 2020-10-08 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **B** |  | | | | | ***Release:*** | | | *Rel-16* |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-15 (Release 15) Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  |  | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  |  | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  |  | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

*Change Start*

#### 4.3.5.X *v2x-SupportedTxBandCombListPerBC-v16xy, v2x-SupportedRxBandCombListPerBC-v16xy*

This field indicates, for a particular band combination of EUTRA, the supported band combination list among *v2x-SupportedBandCombinationListNR* on which the UE supports simultaneous transmission or reception of EUTRA and V2X sidelink communication respectively.

*Next Change*

#### 4.3.21.X *tx-Sidelink-r16, rx-Sidelink-r16*

This parameter indicates whether the UE supports sidelink transmission/reception on the band in the band combination. For NR sidelink transmission, this field is only applicable if the UE supports at least one of sl-TransmissionMode1-r16 and sl-TransmissionMode2-r16 on the band as specified in TS 38.331 [82]. For NR sidelink reception, this field is only applicable if the UE supports sl-Reception-r16 on the band as specified in TS 38.331 [82].

*End of Change*