**3GPP TSG-RAN WG2 Meeting #111-e *R2-2008641***

**E-meeting, 17th – 28th August 2020**

|  |
| --- |
| *CR-Form-v11.2* |
| **CHANGE REQUEST** |
|  |
|  | **38.331** | **CR** | **2007** | **rev** | **-** | **Current version:** | **16.1.0** |  |
|  |
| *For* [*HELP*](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **x** | Radio Access Network | **x** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  |  |
|  |  |
| ***Source to WG:*** | China Telecom, ZTE Corporation, Sanechips, vivo, Apple, Huawei, HiSilicon, OPPO |
| ***Source to TSG:*** | R2 |
|  |  |
| ***Work item code:*** | NR\_RF\_FR1 |  | ***Date:*** | 2020-08-28 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-16 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)* |
|  |  |
| ***Reason for change:*** | 1. Introducing power boosting in UL Tx switching CA case: Accroding to the exception sheet (RP-201379) approved in RAN#88e meeting, one remaining issue in RAN2 is:

|  |
| --- |
| RAN2:* The capability to indicate support of power boosting for CA case, and the RRC signalling to indicate whether such power boosting for CA case is allowed will be specified.
 |

The granularity, definition as well as applicable case of the new UE capability are described in the endorsed WF (RP-201365), see below:

|  |
| --- |
| *#Extracted from RP-201365#*For RAN2, the capability to indicate support of power boosting for CA case, and the RRC signaling to indicate whether such power boosting for CA case is allowed will be specified in Q3, while keep the RAN2 CR pack to this RAN plenary as approved. The capability for 3dB power boosting is defined per band combination. No spec change for RAN2 RRC procedures and MAC procedures. Send the LS to RAN2 in this RAN plenary.…Revise the 38.101-1 CR in RP-200879 to add the indication of 3dB power boosting for carrier 2 with 2Tx for transmission in Case 2, i.e., add the newly proposed text from ZTE.In the CR, the power boosting for carrier 2 with 2Tx is only applied to PC3 CA, i.e., not applied to PC2 CA (the same per BC power class, i.e. PC3 in this case is applied regardless of transmission in Case 1 or Case 2) |

This CR is provided to capture above requirement. 2. In the last RAN2 meeting, it was agreed to clarify the support of NGEN-DC for UE capabilities. However, for the Rel-16 UL Tx switching capabilities applicable to EN-DC (e.g.*ULTxSwitchingBandPair-r16*), it is still unclear whether the capability also applies to NGEN-DC. Hence, this CR aims at clarifying the the support of NGEN-DC for the Rel-16 UL Tx switching UE capabilities that apply to EN-DC. |
|  |  |
| ***Summary of change:*** | 1. Adding new field “ *uplinkTxSwitchingPowerBoosting*” in CellGroupConfig, used to indicate whether the UE is allowed to use 3dB power boosting on carrier2 for UL Tx switching CA case;
2. Adding new UE capability “uplinkTxSwitching-PowerBoosting” in BandCominationList, used to indicate UE’s support of 3dB power boosting on carrier2 for UL Tx switching CA case.
3. Adding the clarification of supporting NGEN-DC in the description of *uplinkTxSwitchingOption, uplinkTxSwitchingPeriodLocation, uplinkTxSwitchingCarrier* and *supportedBandCombinationList-UplinkTxSwitch, uplinkTxSwitchRequest*..

**Impact analysis**Impacted 5G architecture options:NR SA, (NG)EN-DCImpacted functionality:Dynamic UL Tx switchingInter-operability: 1. If the network implements the CR and the UE does not, the UE is unable to report the support of power boosting capability to network, thus network cannot enable the power boosting for UL Tx switching CA case.
2. If the UE implements the CR the network does not, the network cannot decode the power boosting capability and cannot enable the power boosting function for UL Tx switching CA case.
3. If UE implements according to the CR and the network does not, it is unclear for network how to interpret whether the reported UE capability is also supported for NGEN-DC;
4. If the network implements according to the CR and the UE does not, the UE is unable to report related UE capabilities for NGEN-DC. The network may assume those capabilities are not supported by UE in NGEN-DC.
 |
|  |  |
| ***Consequences if not approved:*** | For UE supports UL Tx switching in CA case, the UE is unable to report the support of 3dB power boosting on carrier 2 in case2.It is still unclear whether the configuration and the capability is also applicable to NGEN-DC. |
|  |  |
| ***Clauses affected:*** | 6.3.2, 6.3.3 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** | **x** |  |  Other core specifications  | TS 38.306 CR.. |
| ***affected:*** |  | **x** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **x** |  O&M Specifications | CR  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

Start of changes

### 6.3.2 Radio resource control information elements

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*Unchanged part omittd\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

– *CellGroupConfig*

The *CellGroupConfig* IE is used to configure a master cell group (MCG) or secondary cell group (SCG). A cell group comprises of one MAC entity, a set of logical channels with associated RLC entities and of a primary cell (SpCell) and one or more secondary cells (SCells).

***CellGroupConfig* information element**

-- ASN1START

-- TAG-CELLGROUPCONFIG-START

-- Configuration of one Cell-Group:

CellGroupConfig ::= SEQUENCE {

 cellGroupId CellGroupId,

 rlc-BearerToAddModList SEQUENCE (SIZE(1..maxLC-ID)) OF RLC-BearerConfig OPTIONAL, -- Need N

 rlc-BearerToReleaseList SEQUENCE (SIZE(1..maxLC-ID)) OF LogicalChannelIdentity OPTIONAL, -- Need N

 mac-CellGroupConfig MAC-CellGroupConfig OPTIONAL, -- Need M

 physicalCellGroupConfig PhysicalCellGroupConfig OPTIONAL, -- Need M

 spCellConfig SpCellConfig OPTIONAL, -- Need M

 sCellToAddModList SEQUENCE (SIZE (1..maxNrofSCells)) OF SCellConfig OPTIONAL, -- Need N

 sCellToReleaseList SEQUENCE (SIZE (1..maxNrofSCells)) OF SCellIndex OPTIONAL, -- Need N

 ...,

 [[

 reportUplinkTxDirectCurrent ENUMERATED {true} OPTIONAL -- Cond BWP-Reconfig

 ]],

 [[

 bap-Address-r16 BIT STRING (SIZE (10)) OPTIONAL, -- Need M

 bh-RLC-ChannelToAddModList-r16 SEQUENCE (SIZE(1..maxBH-RLC-ChannelID-r16)) OF BH-RLC-ChannelConfig-r16 OPTIONAL, -- Need N

 bh-RLC-ChannelToReleaseList-r16 SEQUENCE (SIZE(1..maxBH-RLC-ChannelID-r16)) OF BH-RLC-ChannelID-r16 OPTIONAL, -- Need N

 f1c-TransferPath-r16 ENUMERATED {lte, nr, both} OPTIONAL, -- Need M

 simultaneousTCI-UpdateList1-r16 SEQUENCE (SIZE (1..maxNrofServingCellsTCI-r16)) OF ServCellIndex OPTIONAL, -- Need R

 simultaneousTCI-UpdateList2-r16 SEQUENCE (SIZE (1..maxNrofServingCellsTCI-r16)) OF ServCellIndex OPTIONAL, -- Need R

 simultaneousSpatial-UpdatedList1-r16 SEQUENCE (SIZE (1..maxNrofServingCellsTCI-r16)) OF ServCellIndex OPTIONAL, -- Need R

 simultaneousSpatial-UpdatedList2-r16 SEQUENCE (SIZE (1..maxNrofServingCellsTCI-r16)) OF ServCellIndex OPTIONAL, -- Need R

 uplinkTxSwitchingOption-r16 ENUMERATED {switchedUL, dualUL} OPTIONAL -- Need R

 ]] ,

 [[

 uplinkTxSwitchingPowerBoosting-r16 ENUMERATED {enabled} OPTIONAL -- Need R

 ]]

}

-- Serving cell specific MAC and PHY parameters for a SpCell:

SpCellConfig ::= SEQUENCE {

 servCellIndex ServCellIndex OPTIONAL, -- Cond SCG

 reconfigurationWithSync ReconfigurationWithSync OPTIONAL, -- Cond ReconfWithSync

 rlf-TimersAndConstants SetupRelease { RLF-TimersAndConstants } OPTIONAL, -- Need M

 rlmInSyncOutOfSyncThreshold ENUMERATED {n1} OPTIONAL, -- Need S

 spCellConfigDedicated ServingCellConfig OPTIONAL, -- Need M

 ...

}

ReconfigurationWithSync ::= SEQUENCE {

 spCellConfigCommon ServingCellConfigCommon OPTIONAL, -- Need M

 newUE-Identity RNTI-Value,

 t304 ENUMERATED {ms50, ms100, ms150, ms200, ms500, ms1000, ms2000, ms10000},

 rach-ConfigDedicated CHOICE {

 uplink RACH-ConfigDedicated,

 supplementaryUplink RACH-ConfigDedicated

 } OPTIONAL, -- Need N

 ...,

 [[

 smtc SSB-MTC OPTIONAL -- Need S

 ]],

 [[

 daps-UplinkPowerConfig-r16 DAPS-UplinkPowerConfig-r16 OPTIONAL -- Need N

 ]]

}

DAPS-UplinkPowerConfig-r16 ::= SEQUENCE {

 p-DAPS-Source-r16 P-Max,

 p-DAPS-Target-r16 P-Max,

 uplinkPowerSharingDAPS-Mode-r16 ENUMERATED {semi-static-mode1, semi-static-mode2, dynamic }

}

SCellConfig ::= SEQUENCE {

 sCellIndex SCellIndex,

 sCellConfigCommon ServingCellConfigCommon OPTIONAL, -- Cond SCellAdd

 sCellConfigDedicated ServingCellConfig OPTIONAL, -- Cond SCellAddMod

 ...,

 [[

 smtc SSB-MTC OPTIONAL -- Need S

 ]],

 [[

 sCellState-r16 ENUMERATED {activated} OPTIONAL, -- Cond SCellAddSync

 secondaryDRX-GroupConfig-r16 ENUMERATED {true} OPTIONAL -- Cond DRX-Config2

 ]]}

-- TAG-CELLGROUPCONFIG-STOP

-- ASN1STOP

|  |
| --- |
| ***CellGroupConfig* field descriptions** |
| ***bap-Address***BAP address of the parent node in cell group. |
| ***bh-RLC-ChannelToAddModList***Configuration of the backhaul RLC entities and the corresponding MAC Logical Channels to be added and modified. |
| ***bh-RLC-ChannelToReleaseList***List of the backhaul RLC entities and the corresponding MAC Logical Channels to be released. |
| ***f1c-TransferPath***The F1-C transfer path that an EN-DC IAB-MT should use for transferring F1-C packets to the Donor-CU. If IAB-MT is configured with lte, IAB-MT can only use LTE leg for F1-C transfer. If IAB-MT is configured with nr, IAB-MT can only use NR leg for F1-C transfer. If IAB-MT is configured with both, it is up to IAB-MT to select an LTE leg or a NR leg for F1-C transfer. |
| ***mac-CellGroupConfig***MAC parameters applicable for the entire cell group. |
| ***rlc-BearerToAddModList***Configuration of the MAC Logical Channel, the corresponding RLC entities and association with radio bearers. |
| ***reportUplinkTxDirectCurrent***Enables reporting of uplink and supplementary uplink Direct Current location information upon BWP configuration and reconfiguration. This field is only present when the BWP configuration is modified or any serving cell is added or removed. This field is absent in the IE *CellGroupConfig* when provided as part of *RRCSetup* message. If UE is configured with SUL carrier, UE reports both UL and SUL Direct Current locations. |
| ***rlmInSyncOutOfSyncThreshold***BLER threshold pair index for IS/OOS indication generation, see TS 38.133 [14], table 8.1.1-1. *n1* corresponds to the value 1. When the field is absent, the UE applies the value 0. Whenever this is reconfigured, UE resets N310 and N311, and stops T310, if running. Network does not include this field. |
| ***sCellState***Indicates whether the SCell shall be considered to be in activated state upon SCell configuration. |
| ***sCellToAddModList***List of secondary serving cells (SCells) to be added or modified. |
| ***sCellToReleaseList***List of secondary serving cells (SCells) to be released. |
| ***secondaryDRX-GroupConfig***The field is used to indicate whether the SCell belongs to the secondary DRX group. All serving cells in the secondary DRX group shall belong to one Frequency Range and all serving cells in the legacy DRX group shall belong to another Frequency Range. |
| ***simultaneousTCI-UpdateList1, simultaneousTCI-UpdateList2***List of serving cells which can be updated simultaneously for TCI relation with a MAC CE. The *simultaneousTCI-UpdateList1* and *simultaneousTCI-UpdateList2* shall not contain same serving cells. Network should not configure serving cells that are configured with CORESETPoolID=1 in these lists. |
| ***simultaneousSpatial-UpdatedList1, simultaneousSpatial-UpdatedList2***List of serving cells which can be updated simultaneously for spatial relation with a MAC CE. The *simultaneousSpatial-UpdatedList1* and *simultaneousSpatial-UpdatedList2* shall not contain same serving cells. Network should not configure serving cells that are configured with CORESETPoolID=1 in these lists. |
| ***spCellConfig***Parameters for the SpCell of this cell group (PCell of MCG or PSCell of SCG).  |
| ***uplinkTxSwitchingOption***Indicates which option is configured for dynamic UL Tx switching for inter-band UL CA or (NG)EN-DC. The field is set to *switchedUL* if network configures option 1 as specified in TS 38.214 [19], or *dualUL* if network configures option 2 as specified in TS 38.214 [19]. Network always configures UE with a value for this field in inter-band UL CA case and (NG)EN-DC case where UE supports dynamic UL Tx switching. |
|  ***uplinkTxSwitchingPowerBoosting***Indicates whether the UE is allowed to enable 3dB boosting on the maximum output power for transmission on carrier2 under the operation state in which 2-port transmission can be supported on carrier2 for inter-band UL CA case with dynamic UL Tx switching as defined in TS 38.101-1 [15]. Network can only configure this field for UL Tx switching in inter-band UL CA case with power Class 3 as defined in TS 38.101-1 [15]. |

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*Unchanged part omittd\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

– *ServingCellConfig*

The IE *ServingCellConfig* is used to configure (add or modify) the UE with a serving cell, which may be the SpCell or an SCell of an MCG or SCG. The parameters herein are mostly UE specific but partly also cell specific (e.g. in additionally configured bandwidth parts). Reconfiguration between a PUCCH and PUCCHless SCell is only supported using an SCell release and add.

***ServingCellConfig* information element**

-- ASN1START

-- TAG-SERVINGCELLCONFIG-START

ServingCellConfig ::= SEQUENCE {

 tdd-UL-DL-ConfigurationDedicated TDD-UL-DL-ConfigDedicated OPTIONAL, -- Cond TDD

 initialDownlinkBWP BWP-DownlinkDedicated OPTIONAL, -- Need M

 downlinkBWP-ToReleaseList SEQUENCE (SIZE (1..maxNrofBWPs)) OF BWP-Id OPTIONAL, -- Need N

 downlinkBWP-ToAddModList SEQUENCE (SIZE (1..maxNrofBWPs)) OF BWP-Downlink OPTIONAL, -- Need N

 firstActiveDownlinkBWP-Id BWP-Id OPTIONAL, -- Cond SyncAndCellAdd

 bwp-InactivityTimer ENUMERATED {ms2, ms3, ms4, ms5, ms6, ms8, ms10, ms20, ms30,

 ms40,ms50, ms60, ms80,ms100, ms200,ms300, ms500,

 ms750, ms1280, ms1920, ms2560, spare10, spare9, spare8,

 spare7, spare6, spare5, spare4, spare3, spare2, spare1 } OPTIONAL, --Need R

 defaultDownlinkBWP-Id BWP-Id OPTIONAL, -- Need S

 uplinkConfig UplinkConfig OPTIONAL, -- Need M

 supplementaryUplink UplinkConfig OPTIONAL, -- Need M

 pdcch-ServingCellConfig SetupRelease { PDCCH-ServingCellConfig } OPTIONAL, -- Need M

 pdsch-ServingCellConfig SetupRelease { PDSCH-ServingCellConfig } OPTIONAL, -- Need M

 csi-MeasConfig SetupRelease { CSI-MeasConfig } OPTIONAL, -- Need M

 sCellDeactivationTimer ENUMERATED {ms20, ms40, ms80, ms160, ms200, ms240,

 ms320, ms400, ms480, ms520, ms640, ms720,

 ms840, ms1280, spare2,spare1} OPTIONAL, -- Cond ServingCellWithoutPUCCH

 crossCarrierSchedulingConfig CrossCarrierSchedulingConfig OPTIONAL, -- Need M

 tag-Id TAG-Id,

 dummy ENUMERATED {enabled} OPTIONAL, -- Need R

 pathlossReferenceLinking ENUMERATED {spCell, sCell} OPTIONAL, -- Cond SCellOnly

 servingCellMO MeasObjectId OPTIONAL, -- Cond MeasObject

 ...,

 [[

 lte-CRS-ToMatchAround SetupRelease { RateMatchPatternLTE-CRS } OPTIONAL, -- Need M

 rateMatchPatternToAddModList SEQUENCE (SIZE (1..maxNrofRateMatchPatterns)) OF RateMatchPattern OPTIONAL, -- Need N

 rateMatchPatternToReleaseList SEQUENCE (SIZE (1..maxNrofRateMatchPatterns)) OF RateMatchPatternId OPTIONAL, -- Need N

 downlinkChannelBW-PerSCS-List SEQUENCE (SIZE (1..maxSCSs)) OF SCS-SpecificCarrier OPTIONAL -- Need S

 ]],

 [[

 supplementaryUplinkRelease ENUMERATED {true} OPTIONAL, -- Need N

 tdd-UL-DL-ConfigurationDedicated-iab-mt-r16 TDD-UL-DL-ConfigDedicated-IAB-MT-r16 OPTIONAL, -- Cond TDD\_IAB

 dormantBWP-Config-r16 SetupRelease { DormantBWP-Config-r16 } OPTIONAL, -- Need M

 ca-SlotOffset-r16 CHOICE {

 refSCS15kHz INTEGER (-2..2),

 refSCS30KHz INTEGER (-5..5),

 refSCS60KHz INTEGER (-10..10),

 refSCS120KHz INTEGER (-20..20)

 } OPTIONAL, -- Cond AsyncCA

 channelAccessConfig-r16 SetupRelease { ChannelAccessConfig-r16 } OPTIONAL, -- Need M

 intraCellGuardBandsUL-r16 IntraCellGuardBands-r16 OPTIONAL, -- Need S

 intraCellGuardBandsDL-r16 IntraCellGuardBands-r16 OPTIONAL, -- Need S

 csi-RS-ValidationWith-DCI-r16 ENUMERATED {enabled} OPTIONAL, -- Need R

 lte-CRS-PatternList1-r16 SetupRelease { LTE-CRS-PatternList-r16 } OPTIONAL, -- Need M

 lte-CRS-PatternList2-r16 SetupRelease { LTE-CRS-PatternList-r16 } OPTIONAL, -- Need M

 crs-RateMatch-PerCORESETPoolIndex-r16 ENUMERATED {enabled} OPTIONAL, -- Need R

 enableTwoDefaultTCIStates-r16 ENUMERATED {enabled} OPTIONAL, -- Need R

 enableDefaultTCIStatePerCoresetPoolIndex-r16 ENUMERATED {enabled} OPTIONAL, -- Need R

 enableBeamSwitchTiming-r16 ENUMERATED {true} OPTIONAL, -- Need R

 cbg-TxDiffTBsProcessingType1-r16 ENUMERATED {enabled} OPTIONAL, -- Need R

 cbg-TxDiffTBsProcessingType2-r16 ENUMERATED {enabled} OPTIONAL -- Need R

 ]]

}

UplinkConfig ::= SEQUENCE {

 initialUplinkBWP BWP-UplinkDedicated OPTIONAL, -- Need M

 uplinkBWP-ToReleaseList SEQUENCE (SIZE (1..maxNrofBWPs)) OF BWP-Id OPTIONAL, -- Need N

 uplinkBWP-ToAddModList SEQUENCE (SIZE (1..maxNrofBWPs)) OF BWP-Uplink OPTIONAL, -- Need N

 firstActiveUplinkBWP-Id BWP-Id OPTIONAL, -- Cond SyncAndCellAdd

 pusch-ServingCellConfig SetupRelease { PUSCH-ServingCellConfig } OPTIONAL, -- Need M

 carrierSwitching SetupRelease { SRS-CarrierSwitching } OPTIONAL, -- Need M

 ...,

 [[

 powerBoostPi2BPSK BOOLEAN OPTIONAL, -- Need M

 uplinkChannelBW-PerSCS-List SEQUENCE (SIZE (1..maxSCSs)) OF SCS-SpecificCarrier OPTIONAL -- Need S

 ]],

 [[

 enablePLRS-UpdateForPUSCH-SRS-r16 ENUMERATED {enabled} OPTIONAL, -- Need R

 enableDefaultBeamPL-ForPUSCH0-r16 ENUMERATED {enabled} OPTIONAL, -- Need R

 enableDefaultBeamPL-ForPUCCH-r16 ENUMERATED {enabled} OPTIONAL, -- Need R

 enableDefaultBeamPL-ForSRS-r16 ENUMERATED {enabled} OPTIONAL, -- Need R

 uplinkTxSwitching-r16 SetupRelease { UplinkTxSwitching-r16 } OPTIONAL -- Need M

 ]]

}

ChannelAccessConfig-r16 ::= SEQUENCE {

 maxEnergyDetectionThreshold-r16 INTEGER(-85..-52),

 energyDetectionThresholdOffset-r16 INTEGER (-20..-13),

 ul-toDL-COT-SharingED-Threshold-r16 INTEGER (-85..-52) OPTIONAL, -- Need R

 absenceOfAnyOtherTechnology-r16 ENUMERATED {true} OPTIONAL -- Need R

}

IntraCellGuardBands-r16 ::= SEQUENCE (SIZE (1..4)) OF GuardBand-r16

GuardBand-r16 ::= SEQUENCE {

 startCRB-r16 INTEGER (0..274),

 nrofCRBs-r16 INTEGER (0..15)

}

DormancyGroupID-r16 ::= INTEGER (0..4)

DormantBWP-Config-r16::= SEQUENCE {

 dormantBWP-Id-r16 BWP-Id OPTIONAL, -- Need M

 withinActiveTimeConfig-r16 SetupRelease { WithinActiveTimeConfig-r16 } OPTIONAL, -- Need M

 outsideActiveTimeConfig-r16 SetupRelease { OutsideActiveTimeConfig-r16 } OPTIONAL -- Need M

}

WithinActiveTimeConfig-r16 ::= SEQUENCE {

 firstWithinActiveTimeBWP-Id-r16 BWP-Id OPTIONAL, -- Need M

 dormancyGroupWithinActiveTime-r16 DormancyGroupID-r16 OPTIONAL -- Need R

}

OutsideActiveTimeConfig-r16 ::= SEQUENCE {

 firstOutsideActiveTimeBWP-Id-r16 BWP-Id OPTIONAL, -- Need M

 dormancyGroupOutsideActiveTime-r16 DormancyGroupID-r16 OPTIONAL -- Need R

}

UplinkTxSwitching-r16 ::= SEQUENCE {

 uplinkTxSwitchingPeriodLocation-r16 BOOLEAN,

 uplinkTxSwitchingCarrier-r16 ENUMERATED {carrier1, carrier2}

}

-- TAG-SERVINGCELLCONFIG-STOP

-- ASN1STOP

|  |
| --- |
| ***ServingCellConfig* field descriptions** |
| ***absenceOfAnyOtherTechnology***Presence of this field indicates absence on a long term basis (e.g. by level of regulation) of any other technology sharing the carrier; absence of this field indicates the potential presence of any other technology sharing the carrier, as specified in TS 37.213 [48} clause Y. |
| ***bwp-InactivityTimer***The duration in ms after which the UE falls back to the default Bandwidth Part (see TS 38.321 [3], clause 5.15). When the network releases the timer configuration, the UE stops the timer without switching to the default BWP. |
| ***ca-SlotOffset***Slot offset between the primary cell (PCell/PSCell) and the SCell in unaligned frame boundary with slot alignment and partial SFN alignment inter-band CA. Based on this field, the UE determines the time offset of the SCell as specified in clause 4.5 of TS 38.211 [16]. The granularity of this field is determined by the reference SCS for the slot offset (i.e. the maximum of PCell/PSCell lowest SCS among all the configured SCSs in DL/UL *SCS-SpecificCarrierList* in *ServingCellConfig* and this serving cell's lowest SCS among all the configured SCSs in DL/UL *SCS-SpecificCarrierList* in *ServingCellConfig*).The Network configures at most single non-zero offset duration in ms (independent on SCS) among CCs in the unaligned CA configuration. If the field is absent, the UE applies the value of 0. |
| ***cbg-TxDiffTBsProcessingType1, cbg-TxDiffTBsProcessingType2***Indicates whether processing types 1 and 2 based CBG based operation is enabled according to Rel-16 UE capabilities. |
| ***channelAccessConfig***List of parameters used for access procedures of operation with shared spectrum channel access (see TS 37.213 [48). |
| ***crossCarrierSchedulingConfig***Indicates whether this serving cell is cross-carrier scheduled by another serving cell or whether it cross-carrier schedules another serving cell. |
| ***csi-RS-ValidationWith-DCI***Determines how the UE performs periodic and semi-persistent CSI-RS reception in a slot if the UE does not detect a DCI format indicating aperiodic CSI-RS or PDSCH in the set of symbols (see TS 38.213 [13], clause 11.1). |
| ***crs-RateMatch-PerCORESETPoolIndex***Indicates how UE performs rate matching when both lte-CRS-PatternList1-r16 and lte-CRS-PatternList2-r16 are configured as specified in TS 38.314, clause 5.1.4.2. |
| ***defaultDownlinkBWP-Id***The initial bandwidth part is referred to by BWP-Id = 0. ID of the downlink bandwidth part to be used upon expiry of the BWP inactivity timer. This field is UE specific. When the field is absent the UE uses the initial BWP as default BWP. (see TS 38.213 [13], clause 12 and TS 38.321 [3], clause 5.15). |
| ***dormantBWP-Config***The dormant BWP configuration for an SCell. This field can be included only for a (non-PUCCH) SCell. |
| ***downlinkBWP-ToAddModList***List of additional downlink bandwidth parts to be added or modified. (see TS 38.213 [13], clause 12). |
| ***downlinkBWP-ToReleaseList***List of additional downlink bandwidth parts to be released. (see TS 38.213 [13], clause 12). |
| ***downlinkChannelBW-PerSCS-List***A set of UE specific channel bandwidth and location configurations for different subcarrier spacings (numerologies). Defined in relation to Point A. The UE uses the configuration provided in this field only for the purpose of channel bandwidth and location determination. If absent, UE uses the configuration indicated in *scs-SpecificCarrierList* in *DownlinkConfigCommon* / *DownlinkConfigCommonSIB*. Network only configures channel bandwidth that corresponds to the channel bandwidth values defined in TS 38.101-1 [15] and TS 38.101-2 [39]. |
| ***enableBeamSwitchTiming***Indicates the aperiodic CSI-RS triggering with beam switching triggering behaviour as defined in clause 5.2.1.5.1 of TS 38.214 [19]. |
| ***enableDefaultTCIStatePerCoresetPoolIndex***Presence of this field indicates the UE shall follow the release 16 behavior of default TCI state per CORESETPoolindex when the UE is configured by higher layer parameter PDCCH-Config that contains two different values of CORESETPoolIndex in ControlResourceSet is enabled. |
| ***enableTwoDefaultTCIStates***Presence of this field indicates the UE shall follow the release 16 behavior of two default TCI states for PDSCH when at least one TCI codepoint is mapped to two TCI states is enabled |
| ***energyDetectionThresholdOffset***Indicates the offset to the default maximum energy detection threshold value. Unit in dB. Value -13 corresponds to -13dB, value -12 corresponds to -12dB, and so on (i.e. in steps of 1dB) as specified in TS 37.213 [48]. |
| ***firstActiveDownlinkBWP-Id***If configured for an SpCell, this field contains the ID of the DL BWP to be activated upon performing the RRC (re-)configuration. If the field is absent, the RRC (re-)configuration does not impose a BWP switch.If configured for an SCell, this field contains the ID of the downlink bandwidth part to be used upon activation of an SCell. The initial bandwidth part is referred to by BWP-Id = 0.Upon PCell change and PSCell addition/change, the network sets the *firstActiveDownlinkBWP-Id* and *firstActiveUplinkBWP-Id* to the same value. |
| ***initialDownlinkBWP***The dedicated (UE-specific) configuration for the initial downlink bandwidth-part (i.e. DL BWP#0). If any of the optional IEs are configured within this IE, the UE considers the BWP#0 to be an RRC configured BWP (from UE capability viewpoint). Otherwise, the UE does not consider the BWP#0 as an RRC configured BWP (from UE capability viewpoint). Network always configures the UE with a value for this field if no other BWPs are configured. NOTE1 |
| ***intraCellGuardBandsDL, intraCellGuardBandsUL***List of intra-cell guard bands in a serving cell. For each entry in the list, *startCRB* indicates the starting RB of the guard band and *nrofCRBs* indicates the length of the guard band in RBs. For *intraCellGuardBandsUL,* when *nrofCRBs* is 0, zero-size or no guard band is used. If not configured, the guard bands are defined according the TS 38.104 [12] and 38.101-1 [15]. |
| ***lte-CRS-PatternList***A list of LTE CRS patterns around which the UE shall do rate matching for PDSCH. The LTE CRS patterns in this list shall be non-overlapping in frequency. The network does not configure this field and *lte-CRS-ToMatchAround* simultaneously. |
| ***lte-CRS-PatternList2***A list of LTE CRS patterns around which the UE shall do rate matching for PDSCH scheduled with a DCI detected on a CORESET with CORESETPoolIndex configured with 1. This list is configured only if CORESETPoolIndex configured with 1. The first LTE CRS pattern in this list shall be fully overlapping in frequency with the first LTE CRS pattern in lte-CRS-PatternList, The second LTE CRS pattern in this list shall be fully overlapping in frequency with the second LTE CRS pattern in lte-CRS-PatternList, and so on. Network configures this field only if the field *lte-CRS-ToMatchAround* is not configured and there is at least one ControlResourceSet in one DL BWP of this serving cell with *coresetPoolIndex* set to 1. |
| ***lte-CRS-ToMatchAround***Parameters to determine an LTE CRS pattern that the UE shall rate match around. |
| ***maxEnergyDetectionThreshold***Indicates the absolute maximum energy detection threshold value. Unit in dBm. Value -85 corresponds to -85 dBm, value -84 corresponds to -84 dBm, and so on (i.e. in steps of 1dBm) as specified in TS 37.213 [48]. If the field is not configured, the UE shall use a default maximum energy detection threshold value as specified in TS 37.213 [48]. |
| ***pathlossReferenceLinking***Indicates whether UE shall apply as pathloss reference either the downlink of SpCell (PCell for MCG or PSCell for SCG) or of SCell that corresponds with this uplink (see TS 38.213 [13], clause 7). |
| ***pdsch-ServingCellConfig***PDSCH related parameters that are not BWP-specific. |
| ***rateMatchPatternToAddModList***Resources patterns which the UE should rate match PDSCH around. The UE rate matches around the union of all resources indicated in the rate match patterns. Rate match patterns defined here on cell level apply only to PDSCH of the same numerology. See TS 38.214 [19], clause 5.1.2.2.3. |
| ***sCellDeactivationTimer***SCell deactivation timer in TS 38.321 [3]. If the field is absent, the UE applies the value infinity. |
| ***servingCellMO****measObjectId* of the *MeasObjectNR* in *MeasConfig* which is associated to the serving cell. For this *MeasObjectNR*, the following relationship applies between this MeasObjectNR and *frequencyInfoDL* in *ServingCellConfigCommon* of the serving cell: if *ssbFrequency* is configured, its value is the same as the *absoluteFrequencySSB* and if *csi-rs-ResourceConfigMobility* is configured, the value of its *subcarrierSpacing* is present in one entry of the *scs-SpecificCarrierList*, *csi-RS-CellListMobility* includes an entry corresponding to the serving cell (with *cellId* equal to *physCellId* in *ServingCellConfigCommon*) and the frequency range indicated by the *csi-rs-MeasurementBW* of the entry in *csi-RS-CellListMobility* is included in the frequency range indicated by in the entry of the *scs-SpecificCarrierList*.  |
| ***supplementaryUplink***Network may configure this field only when *supplementaryUplinkConfig* is configured in *ServingCellConfigCommon* or *ServingCellConfigCommonSIB*. |
| ***supplementaryUplinkRelease***If this field is included, the UE shall release the uplink configuration configured by *supplementaryUplink*. The network only includes either *supplementaryUplinkRelease* or *supplementaryUplink* at a time. |
| ***tag-Id***Timing Advance Group ID, as specified in TS 38.321 [3], which this cell belongs to. |
| ***tdd-UL-DL-ConfigurationDedicated-iab-mt***Resource configuration per IAB-MT D/U/F overrides all symbols (with a limitation that effectively only flexible symbols can be overwritten in Rel-16) per slot over the number of slots as provided by *TDD-UL-DL ConfigurationCommon*. |
| ***ul-toDL-COT-SharingED-Threshold***Maximum energy detection threshold that the UE should use to share channel occupancy with gNB for DL transmission with length no longer than 2, 4, and 8 OFDM symbols for 15Khz, 30Khz, 60KHz SCS respectively, as specified in TS 37.213 [48]. |
| ***uplinkConfig***Network may configure this field only when *uplinkConfigCommon* is configured in *ServingCellConfigCommon* or *ServingCellConfigCommonSIB*. Addition or release of this field can only be done upon SCell addition or release (respectively). |

|  |
| --- |
| ***UplinkConfig* field descriptions** |
| ***carrierSwitching***Includes parameters for configuration of carrier based SRS switching (see TS 38.214 [19], clause 6.2.1.3. |
| ***enableDefaultBeamPlForPUSCH0\_0, enableDefaultBeamPlForPUCCH, enableDefaultBeamPlForSRS***When the parameter is present, UE derives the spatial relation and the corresponding pathloss reference Rs as specified in 38.213, clauses 7.1.1, 7.2.1, 7.3.1 and 9.2.2The network only configures these parameters for FR2. |
| ***enablePLRSupdateForPUSCHSRS***When this parameter is present, the Rel-16 feature of MAC CE based pathloss RS updates for PUSCH/SRS is enabled. Network only configures this parameter , when the UE is configured with *sri-PUSCH-PowerControl*. |
| ***firstActiveUplinkBWP-Id***If configured for an SpCell, this field contains the ID of the UL BWP to be activated upon performing the RRC (re-)configuration. If the field is absent, the RRC (re-)configuration does not impose a BWP switch.If configured for an SCell, this field contains the ID of the uplink bandwidth part to be used upon MAC-activation of an SCell. The initial bandwidth part is referred to by BandiwdthPartId = 0. |
| ***initialUplinkBWP***The dedicated (UE-specific) configuration for the initial uplink bandwidth-part (i.e. UL BWP#0). If any of the optional IEs are configured within this IE as part of the IE *uplinkConfig*, the UE considers the BWP#0 to be an RRC configured BWP (from UE capability viewpoint). Otherwise, the UE does not consider the BWP#0 as an RRC configured BWP (from UE capability viewpoint). Network always configures the UE with a value for this field if no other BWPs are configured. NOTE1 |
| ***powerBoostPi2BPSK***If this field is set to *true*, the UE determines the maximum output power for PUCCH/PUSCH transmissions that use pi/2 BPSK modulation according to TS 38.101-1 [15], clause 6.2.4. |
| ***pusch-ServingCellConfig***PUSCH related parameters that are not BWP-specific. |
| ***uplinkBWP-ToAddModList***The additional bandwidth parts for uplink to be added or modified. In case of TDD uplink- and downlink BWP with the same *bandwidthPartId* are considered as a BWP pair and must have the same center frequency. |
| ***uplinkBWP-ToReleaseList***The additional bandwidth parts for uplink to be released. |
| ***uplinkChannelBW-PerSCS-List***A set of UE specific channel bandwidth and location configurations for different subcarrier spacings (numerologies). Defined in relation to Point A. The UE uses the configuration provided in this field only for the purpose of channel bandwidth and location determination. If absent, UE uses the configuration indicated in *scs-SpecificCarrierList* in *UplinkConfigCommon* / *UplinkConfigCommonSIB*. Network only configures channel bandwidth that corresponds to the channel bandwidth values defined in TS 38.101-1 [15] and TS 38.101-2 [39]. |
| ***uplinkTxSwitchingPeriodLocation***Indicates whether the location of UL Tx switching period is configured in this uplink carrier in case of inter-band UL CA, SUL, or (NG)EN-DC, as specified in TS 38.101-1 [15] and TS 38.101-3 [34]. In case of inter-band UL CA or SUL, network configures this field to TRUE for one of the uplink carriers involved in dynamic UL TX switching and configures this field in the other carrier to FALSE. In case of (NG)EN-DC, network always configures this field to TRUE for NR carrier (i.e. with (NG)EN-DC, the UL switching period always occurs on the NR carrier). |
| ***uplinkTxSwitchingCarrier***Indicates that the configured carrier is carrier1 or carrier2 for dynamic uplink Tx switching, as defined in TS 38.101-1 [15] and TS 38.101-3 [34]. In case of inter-band UL CA or SUL, network configures one of the two uplink carriers involved in dynamic UL TX switching as carrier1 and the other as carrier2. In case of (NG)EN-DC, network always configures the NR carrier as carrier 2. |

|  |
| --- |
| ***DormantBWP-Config* field descriptions** |
| ***dormancyGroupWithinActiveTime***This field contains the ID of an SCell group for Dormancy within active time, to which this SCell belongs. The use of the Dormancy within active time SCell groups is specified in TS 38.213 [13]. |
| ***dormancyGroupOutsideActiveTime***This field contains the ID of an SCell group for Dormancy outside active time, to which this SCell belongs. The use of the Dormancy outside active time SCell groups is specified in TS 38.213 [13]. |
| ***dormantBWP-Id***This field contains the ID of the downlink bandwidth part to be used as dormant BWP. If this field is configured, its value is different from *defaultDownlinkBWP-Id*, and at least one of the *withinActiveTimeConfig* and *outsideActiveTimeConfig* should be configured. |
| ***firstOutsideActiveTimeBWP-Id***This field contains the ID of the downlink bandwidth part to be activated when receiving a DCI indication for SCell dormancy outside active time. |
| ***firstWithinActiveTimeBWP-Id***This field contains the ID of the downlink bandwidth part to be activated when receiving a DCI indication for SCell dormancy within active time. |
| ***outsideActiveTimeConfig***This field contains the configuration to be used for SCell dormancy outside active time, as specified in TS 38.213 [13]. The field can only be present when the cell group the SCell belongs to is configured with *dcp-Config*. |
| ***withinActiveTimeConfig***This field contains the configuration to be used for SCell dormancy within active time, as specified in TS 38.213 [13].  |

NOTE 1: If the dedicated part of initial UL/DL BWP configuration is absent, the initial BWP can be used but with some limitations. For example, changing to another BWP requires *RRCReconfiguration* since DCI format 1\_0 doesn't support DCI-based switching.

|  |  |
| --- | --- |
| **Conditional Presence** | **Explanation** |
| *AsyncCA* | This field is mandatory present for SCells whose slot offset between the SpCell is not 0. Otherwise it is absent, Need S. |
| *MeasObject* | This field is mandatory present for the SpCell if the UE has a *measConfig*, and it is optionally present, Need M, for SCells. |
| *SCellOnly* | This field is optionally present, Need R, for SCells. It is absent otherwise.  |
| *ServingCellWithoutPUCCH* | This field is optionally present, Need S, for SCells except PUCCH SCells. It is absent otherwise. |
| *SyncAndCellAdd* | This field is mandatory present for a SpCell upon PCell change and PSCell addition/change and upon *RRCSetup*/*RRCResume*.The field is mandatory present for an SCell upon addition.For SpCell, the field is optionally present, Need N, upon reconfiguration without *reconfigurationWithSync*.In all other cases the field is absent. |
| *TDD* | This field is optionally present, Need R, for TDD cells. It is absent otherwise. |
| *TDD\_IAB* | For IAB-MT, this field is optionally present, Need R, for TDD cells. It is absent otherwise. |

Next change

### 6.3.3 UE capability information elements

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*Unchanged part omittd\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

– *BandCombinationList*

The IE *BandCombinationList* contains a list of NR CA and/or MR-DC band combinations (also including DL only or UL only band).

***BandCombinationList* information element**

-- ASN1START

-- TAG-BANDCOMBINATIONLIST-START

BandCombinationList ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination

BandCombinationList-v1540 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v1540

BandCombinationList-v1550 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v1550

BandCombinationList-v1560 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v1560

BandCombinationList-v1570 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v1570

BandCombinationList-v1580 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v1580

BandCombinationList-v1590 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v1590

BandCombinationList-v1610 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v1610

BandCombinationList-UplinkTxSwitch-r16 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-UplinkTxSwitch-r16

BandCombination ::= SEQUENCE {

 bandList SEQUENCE (SIZE (1..maxSimultaneousBands)) OF BandParameters,

 featureSetCombination FeatureSetCombinationId,

 ca-ParametersEUTRA CA-ParametersEUTRA OPTIONAL,

 ca-ParametersNR CA-ParametersNR OPTIONAL,

 mrdc-Parameters MRDC-Parameters OPTIONAL,

 supportedBandwidthCombinationSet BIT STRING (SIZE (1..32)) OPTIONAL,

 powerClass-v1530 ENUMERATED {pc2} OPTIONAL

}

BandCombination-v1540::= SEQUENCE {

 bandList-v1540 SEQUENCE (SIZE (1..maxSimultaneousBands)) OF BandParameters-v1540,

 ca-ParametersNR-v1540 CA-ParametersNR-v1540 OPTIONAL

}

BandCombination-v1550 ::= SEQUENCE {

 ca-ParametersNR-v1550 CA-ParametersNR-v1550

}

BandCombination-v1610 ::= SEQUENCE {

 bandList-v1610 SEQUENCE (SIZE (1..maxSimultaneousBands)) OF BandParameters-v1610 OPTIONAL,

 ca-ParametersNR-v1610 CA-ParametersNR-v1610 OPTIONAL,

 ca-ParametersNRDC-v1610 CA-ParametersNRDC-v1610 OPTIONAL,

 powerClass-v1610 ENUMERATED {pc1dot5} OPTIONAL

}

BandCombination-v1560::= SEQUENCE {

 ne-DC-BC ENUMERATED {supported} OPTIONAL,

 ca-ParametersNRDC CA-ParametersNRDC OPTIONAL,

 ca-ParametersEUTRA-v1560 CA-ParametersEUTRA-v1560 OPTIONAL,

 ca-ParametersNR-v1560 CA-ParametersNR-v1560 OPTIONAL

}

BandCombination-v1570 ::= SEQUENCE {

 ca-ParametersEUTRA-v1570 CA-ParametersEUTRA-v1570

}

BandCombination-v1580 ::= SEQUENCE {

 mrdc-Parameters-v1580 MRDC-Parameters-v1580

}

BandCombination-v1590::= SEQUENCE {

 supportedBandwidthCombinationSetIntraENDC BIT STRING (SIZE (1..32)) OPTIONAL,

 mrdc-Parameters-v1590 MRDC-Parameters-v1590

}

BandCombination-UplinkTxSwitch-r16 ::= SEQUENCE {

 bandCombination-r16 BandCombination,

 bandCombination-v1540 BandCombination-v1540 OPTIONAL,

 bandCombination-v1560 BandCombination-v1560 OPTIONAL,

 bandCombination-v1570 BandCombination-v1570 OPTIONAL,

 bandCombination-v1580 BandCombination-v1580 OPTIONAL,

 bandCombination-v1590 BandCombination-v1590 OPTIONAL,

 bandCombination-v1610 BandCombination-v1610 OPTIONAL,

 supportedBandPairListNR-r16 SEQUENCE (SIZE (1..maxULTxSwitchingBandPairs)) OF ULTxSwitchingBandPair-r16,

 uplinkTxSwitching-OptionSupport-r16 ENUMERATED {switchedUL, dualUL, both} OPTIONAL,

 uplinkTxSwitching-PowerBoosting-r16 ENUMERATED {supported} OPTIONAL,

 ...

}

ULTxSwitchingBandPair-r16 ::= SEQUENCE {

 bandIndexUL1-r16 INTEGER(1..maxSimultaneousBands),

 bandIndexUL2-r16 INTEGER(1..maxSimultaneousBands),

 uplinkTxSwitchingPeriod-r16 ENUMERATED {n35us, n140us, n210us},

 uplinkTxSwitching-DL-Interruption-r16 BIT STRING (SIZE(1..maxSimultaneousBands)) OPTIONAL

}

BandParameters ::= CHOICE {

 eutra SEQUENCE {

 bandEUTRA FreqBandIndicatorEUTRA,

 ca-BandwidthClassDL-EUTRA CA-BandwidthClassEUTRA OPTIONAL,

 ca-BandwidthClassUL-EUTRA CA-BandwidthClassEUTRA OPTIONAL

 },

 nr SEQUENCE {

 bandNR FreqBandIndicatorNR,

 ca-BandwidthClassDL-NR CA-BandwidthClassNR OPTIONAL,

 ca-BandwidthClassUL-NR CA-BandwidthClassNR OPTIONAL

 }

}

BandParameters-v1540 ::= SEQUENCE {

 srs-CarrierSwitch CHOICE {

 nr SEQUENCE {

 srs-SwitchingTimesListNR SEQUENCE (SIZE (1..maxSimultaneousBands)) OF SRS-SwitchingTimeNR

 },

 eutra SEQUENCE {

 srs-SwitchingTimesListEUTRA SEQUENCE (SIZE (1..maxSimultaneousBands)) OF SRS-SwitchingTimeEUTRA

 }

 } OPTIONAL,

 srs-TxSwitch SEQUENCE {

 supportedSRS-TxPortSwitch ENUMERATED {t1r2, t1r4, t2r4, t1r4-t2r4, t1r1, t2r2, t4r4, notSupported},

 txSwitchImpactToRx INTEGER (1..32) OPTIONAL,

 txSwitchWithAnotherBand INTEGER (1..32) OPTIONAL

 } OPTIONAL

}

BandParameters-v1610 ::= SEQUENCE {

 srs-TxSwitch-v1610 SEQUENCE {

 supportedSRS-TxPortSwitch-v1610 ENUMERATED {t1r1-t1r2, t1r1-t1r2-t1r4, t1r1-t1r2-t2r2-t2r4, t1r1-t1r2-t2r2-t1r4-t2r4,

 t1r1-t2r2, t1r1-t2r2-t4r4}

 } OPTIONAL,

 intraFreqDAPS-Parameters-r16 SEQUENCE {

 intraFreqDiffSCS-DAPS-r16 ENUMERATED {supported} OPTIONAL,

 intraFreqDAPS-r16 ENUMERATED {supported} OPTIONAL,

 intraFreqAsyncDAPS-r16 ENUMERATED {supported} OPTIONAL,

 intraFreqMultiUL-TransmissionDAPS-r16 ENUMERATED {supported} OPTIONAL,

 intraFreqTwoTAGs-DAPS-r16 ENUMERATED {supported} OPTIONAL,

 intraFreqSemiStaticPowerSharingDAPS-Mode1-r16 ENUMERATED {supported} OPTIONAL,

 intraFreqSemiStaticPowerSharingDAPS-Mode2-r16 ENUMERATED {supported} OPTIONAL,

 intraFreqDynamicPowersharingDAPS-r16 ENUMERATED {short, long} OPTIONAL

 } OPTIONAL

}

-- TAG-BANDCOMBINATIONLIST-STOP

-- ASN1STOP

|  |
| --- |
| ***BandCombination* field descriptions** |
| ***BandCombinationList-v1540, BandCombinationList-v1550, BandCombinationList-v1560, BandCombinationList-v1570, BandCombinationList-v1580, BandCombinationList-v1590, BandCombinationList-r16***The UE shall include the same number of entries, and listed in the same order, as in *BandCombinationList* (without suffix). If the field is included in *supportedBandCombinationListNEDC-Only-v1610*, the UE shall include the same number of entries, and listed in the same order, as in *BandCombinationList* of *supportedBandCombinationListNEDC-Only* (without suffix) field.If the field is included in *supportedBandCombinationListNEDC-Only-v15a0*, the UE shall include the same number of entries, and listed in the same order, as in *BandCombinationList* (without suffix) of *supportedBandCombinationListNEDC-Only* (without suffix) field. |
| ***ca-ParametersNRDC***If the field is included for a band combination in the NR capability container, the field indicates support of NR-DC. Otherwise, the field is absent. |
| ***ne-DC-BC***If the field is included for a band combination in the MR-DC capability container, the field indicates support of NE-DC. Otherwise, the field is absent. |
| ***srs-SwitchingTimesListNR***Indicates, for a particular pair of NR bands, the RF retuning time when switching between a NR carrier corresponding to this band entry and another (PUSCH-less) NR carrier corresponding to the band entry in the order indicated below:- For the first NR band, the UE shall include the same number of entries for NR bands as in *bandList*, i.e. first entry corresponds to first NR band in *bandList* and so on,- For the second NR band, the UE shall include one entry less, i.e. first entry corresponds to the second NR band in *bandList* and so on- And so on |
| ***srs-SwitchingTimesListEUTRA***Indicates, for a particular pair of E-UTRA bands, the RF retuning time when switching between an E-UTRA carrier corresponding to this band entry and another (PUSCH-less) E-UTRA carrier corresponding to the band entry in the order indicated below:- For the first E-UTRA band, the UE shall include the same number of entries for E-UTRA bands as in *bandList,* i.e. first entry corresponds to first E-UTRA band in *bandList* and so on,- For the second E-UTRA band, the UE shall include one entry less, i.e. first entry corresponds to the second E-UTRA band in *bandList* and so on - And so on |
| ***srs-TxSwitch***Indicates supported SRS antenna switch capability for the associated band. If the UE indicates support of *SRS-SwitchingTimeNR*, the UE is allowed to set this field for a band with associated *FeatureSetUplinkId* set to 0 for SRS carrier switching. |

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*Unchanged part omittd\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

#### – *RF-ParametersMRDC*

The IE *RF-ParametersMRDC* is used to convey RF related capabilities for MR-DC.

*RF-ParametersMRDC* information element

-- ASN1START

-- TAG-RF-PARAMETERSMRDC-START

RF-ParametersMRDC ::= SEQUENCE {

 supportedBandCombinationList BandCombinationList OPTIONAL,

 appliedFreqBandListFilter FreqBandList OPTIONAL,

 ...,

 [[

 srs-SwitchingTimeRequested ENUMERATED {true} OPTIONAL,

 supportedBandCombinationList-v1540 BandCombinationList-v1540 OPTIONAL

 ]],

 [[

 supportedBandCombinationList-v1550 BandCombinationList-v1550 OPTIONAL

 ]],

 [[

 supportedBandCombinationList-v1560 BandCombinationList-v1560 OPTIONAL,

 supportedBandCombinationListNEDC-Only BandCombinationList OPTIONAL

 ]],

 [[

 supportedBandCombinationList-v1570 BandCombinationList-v1570 OPTIONAL

 ]],

 [[

 supportedBandCombinationList-v1580 BandCombinationList-v1580 OPTIONAL

 ]],

 [[

 supportedBandCombinationList-v1590 BandCombinationList-v1590 OPTIONAL

 ]],

 [[

 supportedBandCombinationListNEDC-Only-v15a0 SEQUENCE {

 supportedBandCombinationList-v1540 BandCombinationList-v1540 OPTIONAL,

 supportedBandCombinationList-v1560 BandCombinationList-v1560 OPTIONAL,

 supportedBandCombinationList-v1570 BandCombinationList-v1570 OPTIONAL,

 supportedBandCombinationList-v1580 BandCombinationList-v1580 OPTIONAL,

 supportedBandCombinationList-v1590 BandCombinationList-v1590 OPTIONAL

 } OPTIONAL

 ]],

 [[

 supportedBandCombinationList-v1610 BandCombinationList-v1610 OPTIONAL,

 supportedBandCombinationListNEDC-Only-v1610 BandCombinationList-v1610 OPTIONAL,

 supportedBandCombinationList-UplinkTxSwitch-r16 BandCombinationList-UplinkTxSwitch-r16 OPTIONAL

 ]]

}

-- TAG-RF-PARAMETERSMRDC-STOP

-- ASN1STOP

|  |
| --- |
| *RF-ParametersMRDC* field descriptions |
| ***appliedFreqBandListFilter***In this field the UE mirrors the *FreqBandList* that the NW provided in the capability enquiry, if any. The UE filtered the band combinations in the *supportedBandCombinationList* in accordance with this *appliedFreqBandListFilter*. |
| ***supportedBandCombinationList***A list of band combinations that the UE supports for (NG)EN-DC, or both (NG)EN-DC and NE-DC. The *FeatureSetCombinationId*:s in this list refer to the *FeatureSetCombination* entries in the *featureSetCombinations* list in the *UE-MRDC-Capability* IE. |
| ***supportedBandCombinationListNEDC-Only, supportedBandCombinationListNEDC-Only-v1610***A list of band combinations that the UE supports only for NE-DC. The *FeatureSetCombinationId*:s in this list refer to the *FeatureSetCombination* entries in the *featureSetCombinations* list in the *UE-MRDC-Capability* IE. |
| ***supportedBandCombinationList-UplinkTxSwitch***A list of band combinations that the UE supports dynamic UL Tx switching for (NG)EN-DC. The *FeatureSetCombinationId*:s in this list refer to the *FeatureSetCombination* entries in the *featureSetCombinations* list in the *UE-MRDC-Capability* IE. |

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*Unchanged part omittd\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

#### – *UE-CapabilityRequestFilterCommon*

The IE *UE-CapabilityRequestFilterCommon* is used to request filtered UE capabilities. The filter is common for all capability containers that are requested.

*UE-CapabilityRequestFilterCommon* information element

-- ASN1START

-- TAG-UE-CAPABILITYREQUESTFILTERCOMMON-START

UE-CapabilityRequestFilterCommon ::= SEQUENCE {

 mrdc-Request SEQUENCE {

 omitEN-DC ENUMERATED {true} OPTIONAL, -- Need N

 includeNR-DC ENUMERATED {true} OPTIONAL, -- Need N

 includeNE-DC ENUMERATED {true} OPTIONAL -- Need N

 } OPTIONAL, -- Need N

 ...,

 [[

 codebookTypeRequest-r16 SEQUENCE {

 type1-SinglePanel-r16 ENUMERATED {true} OPTIONAL, -- Need N

 type1-MultiPanel-r16 ENUMERATED {true} OPTIONAL, -- Need N

 type2-r16 ENUMERATED {true} OPTIONAL, -- Need N

 type2-PortSelection-r16 ENUMERATED {true} OPTIONAL -- Need N

 } OPTIONAL, -- Need N

 uplinkTxSwitchRequest-r16 ENUMERATED {true} OPTIONAL -- Need N

 ]]

}

-- TAG-UE-CAPABILITYREQUESTFILTERCOMMON-STOP

-- ASN1STOP

|  |
| --- |
| *UE-CapabilityRequestFilterCommon field descriptions* |
| ***codebookTypeRequest***Only if this field is present, the UE includes *SupportedCSI-RS-Resource* supported for the codebook type(s) requested within this field (i.e. type I single/multi-panel, type II and type II port selection) into *codebookVariantsList*, *codebookParametersPerBand* and *codebookParametersPerBC*. If this field is present and none of the codebook types is requested within this field (i.e. empty field), the UE includes *SupportedCSI-RS-Resource* supported for all codebook types into *codebookVariantsList*, *codebookParametersPerBand* and *codebookParametersPerBC*. |
| ***includeNE-DC***Only if this field is present, the UE supporting NE-DC shall indicate support for NE-DC in band combinations and include feature set combinations which are applicable to NE-DC. Band combinations supporting both NE-DC and (NG)EN-DC shall be included in *supportedBandCombinationList*, band combinations supporting only NE-DC shall be included in *supportedBandCombinationListNEDC-Only*. |
| ***includeNR-DC***Only if this field is present, the UE supporting NR-DC shall indicate support for NR-DC in band combinations and include feature set combinations which are applicable to NR-DC. |
| ***omitEN-DC***Only if this field is present, the UE shall omit band combinations and feature set combinations which are only applicable to (NG)EN-DC. |
| ***uplinkTxSwitchRequest***Only if this field is present, the UE supporting dynamic UL Tx switching shall indicate support for UL Tx switching in band combinations which are applicable to inter-band UL CA, SUL and (NG)EN-DC. |

End of changes