3GPP TSG-RAN WG2 #111-e Draft R2-20xxxxx

Electronic Meeting, August 17 - 28, 2020

Agenda Item: x.x.x

Source: Swift Navigation

Title: [Post111-e][626][POS] Email Discussion on integrity use cases and specification impacts

Document for: Discussion, Decision

# 1 Introduction

This document addresses the agreements, open issues and draft TP for the following email discussion:

* [Post111-e][626][POS] Integrity use cases and specification impacts (Swift)

Scope: Capture any additional integrity use cases and open issues on integrity, and draft a TP incorporating the existing agreements and any further progress.

Intended outcome: Summary to next meeting

Deadline: Long

The agreements from RAN2#111-e are provided below [1]:

**Agreements:**

1. Agree to adopt the Target Integrity Risk (TIR), Alert Limit (AL) and Time-to-Alert TTA) as the Integrity KPIs.

2. Agree to the following definitions of the KPIs:

**Target Integrity Risk (TIR):** The probability that the positioning error exceeds the Alert Limit (AL) without warning the user within the required Time-to-Alert (TTA).

NOTE: The TIR is usually defined as a probability rate per some time unit (e.g. per hour, per second or per independent sample).

**Alert Limit (AL):** The maximum allowable positioning error such that the positioning system is available for the intended application. If the positioning error is beyond the AL, operations are hazardous and the positioning system should be declared unavailable for the intended application to prevent loss of integrity.

NOTE: When the AL bounds the positioning error in the horizontal plane or on the vertical axis then it is called Horizontal Alert Limit (HAL) or Vertical Alert Limit (VAL) respectively.

**Time-to-Alert (TTA):** The maximum allowable elapsed time from when the positioning error exceeds the Alert Limit (AL) until the function providing position integrity annunciates a corresponding alert.

3. Agree to include the PL integrity definition with the following baseline; FFS if updates are needed.

**Protection Level:** The PL is a statistical upper-bound of the positioning error that ensures that, the probability per unit of time of the true error being greater than the AL and the PL being less than or equal to the AL, for longer than the TTA, is less than the required TIR.

NOTE: When the PL bounds the positioning error in the horizontal plane or on the vertical axis then it is called Horizontal Protection Level (HPL) or Vertical Protection Level (VPL) respectively.

4. The additional definitions are FFS on a ‘need-to-define’ basis.

5. Agree to study the Automotive, IIoT and Rail use cases as illustrative examples.

6. Agree to the Skeleton for Section 9 of TR 38.857.

The agreements have been included in the draft text proposal in Section 3 below. The open issues are further discussed in Section 2 below, providing additional considerations for the draft TP.

# 2 Open Issues

The following open issues are presented for discussion and inclusion in the draft TP.

2.1 Use Cases

Three use cases were agreed as illustrative examples of integrity in the draft TP – Automotive, IIoT and Rail [1]. Companies are asked to comment and/or provide suggested text for the TP, with a view to describing the application of integrity to these use cases in accordance with the study objectives.

|  |  |
| --- | --- |
| **Company** | **Please comment on the integrity use case descriptions (Automotive, IIoT, Rail)** |
| Swift Navigation | For the **Automotive** use case, we propose to adopt the Road-Level and Lane-Level Identification text provided in **Section 9.4.1** of [RP-2006541](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_111-e/Docs/R2-2006541.zip) [2], to illustrate the integrity KPIs and core integrity concepts in practice. |

2.2 Protocol Impacts

There was general consensus in the email discussions to review the protocol impacts to the RAN positioning specifications in the SI, in order to inform potential changes as part of the subsequent WI. The following table is therefore proposed for inclusion in Section 9.5 of the draft TP below. Protocol impacts to other specification groups (e.g. SA, CT, OMA) can be considered if a need is identified through the SI findings.

-------------------------------------------------Start of text proposal------------------------------------------------

|  |  |  |  |
| --- | --- | --- | --- |
| **Impacted TS/TR** | | | |
| TS/TR | Vers | Title | Remarks |
| TS 38.305 |  | Stage 2 functional specification of User Equipment (UE) positioning in NG-RAN |  |
| TS 38.331 |  | NR; Radio Resource Control (RRC); Protocol specification |  |
| TS 37.355 |  | LTE Positioning Protocol (LPP) |  |
| TS 38.455 |  | NR Positioning Protocol A (NRPPa) |  |

Table 9.5 – Impacted RAN specifications.

--------------------------------------------------End of text proposal------------------------------------------------

Companies are asked to comment if they agree with the table of specifications.

|  |  |
| --- | --- |
| **Company** | **Do you agree with the specification list for the SI phase?** |
| Swift Navigation | Yes. |

2.3 Integrity Concepts

The Tdoc submissions and email discussions contained information and questions relating to the core integrity concepts and how these concepts will be interpreted and defined within the 3GPP system. The core integrity concepts are therefore important inputs for addressing the remaining objectives (e.g. to categorize the errors, to specify the integrity methodologies, to identify the protocol impacts and to support the definition of more ‘3GPP-friendly’ descriptions throughout the SI/WI). Companies are asked to comment on key topics to be addressed in the integrity concepts.

|  |  |
| --- | --- |
| **Company** | **Please identify the integrity concepts to be considered in the study** |
| Swift Navigation | We believe the Integrity Concepts (Section 9.1.2 of the Skeleton TR) should cover the following topics:   1. **What is positioning integrity?** 2. **Interpretation and relationship between the Protection Level and KPIs.**    * Including the Stanford Diagram conceptual framework.   We think (1) and (2) can be addressed in part by including the text and diagrams from **Section** **9.2.3** (Accuracy versus Integrity), **Section 9.3.1** (KPI Descriptions), and **Section** **9.3.2** (Stanford Diagram) in [RP-2006541](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_111-e/Docs/R2-2006541.zip) [2]. |

# 3 Text Proposal

The following section incorporates the existing agreements as text proposals within the agreed Skeleton.

-------------------------------------------------Start of text proposal------------------------------------------------

9 Positioning integrity and reliability

*From objective 2: Includes solutions necessary to support integrity and reliability of assistance data and position information:*

9.1 Integrity Overview – Background Information

9.1.1 Integrity Definitions

**Target Integrity Risk (TIR):** The probability that the positioning error exceeds the Alert Limit (AL) without warning the user within the required Time-to-Alert (TTA).

NOTE: The TIR is usually defined as a probability rate per some time unit (e.g. per hour, per second or per independent sample).

**Alert Limit (AL):** The maximum allowable positioning error such that the positioning system is available for the intended application. If the positioning error is beyond the AL, operations are hazardous and the positioning system should be declared unavailable for the intended application to prevent loss of integrity.

NOTE: When the AL bounds the positioning error in the horizontal plane or on the vertical axis then it is called Horizontal Alert Limit (HAL) or Vertical Alert Limit (VAL) respectively.

**Time-to-Alert (TTA):** The maximum allowable elapsed time from when the positioning error exceeds the Alert Limit (AL) until the function providing position integrity annunciates a corresponding alert.

**Protection Level:** The PL is a statistical upper-bound of the positioning error that ensures that, the probability per unit of time of the true error being greater than the AL and the PL being less than or equal to the AL, for longer than the TTA, is less than the required TIR.

NOTE: When the PL bounds the positioning error in the horizontal plane or on the vertical axis then it is called Horizontal Protection Level (HPL) or Vertical Protection Level (VPL) respectively.

9.1.2 Integrity Concepts

[TBC in Section 2 - Open Issues]

9.2 Use Cases

9.2.1 Automotive

[TBC in Section 2 - Open Issues]

9.2.2 Industrial IoT

[TBC in Section 2 - Open Issues]

9.2.3 Rail

[TBC in Section 2 - Open Issues]

9.3 Positioning Integrity Error Categories

9.3.1 RAT-Independent

9.3.2 RAT-Dependent

9.4 Positioning Integrity Methods

9.4.1 RAT-Independent

9.4.2 RAT-Dependent

9.5 Procedure and protocol impact analysis

[TBC in Section 2 - Open Issues]

--------------------------------------------------End of text proposal------------------------------------------------

Please provide any additional comments on the text proposal:

|  |  |
| --- | --- |
| **Company** | **Comment** |
|  |  |

# 4 Conclusion

# 5 References

1. [R2-2008125](http://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_111-e/Docs/R2-2008125.zip), Report from session on positioning and sidelink relay, Session Chair (MediaTek).
2. [R2-2006541](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_111-e/Docs/R2-2006541.zip), TP for Study on Positioning Integrity and Reliability, Swift Navigation, Deutsche Telekom, u-blox, Ericsson, Mitsubishi Electric, Intel Corporation, CATT, UIC.