**‎3GPP TSG-RAN WG2 Meeting #111 electronicR2-20xxxxx**

**Online, August 17th - 28th, 2020‎**

**Agenda item: 6.4.2**

**Source: CATT**

**Title: ‎Discussion paper on [Post111-e][701][V2X] 38.304 and 36.304 corrections‎**

**Document for: Discussion and Agreement**

# 1 Introduction

This is to report the result of the following email discussion after RAN2#111-e Meeting [1].

* [POST111-e][701][V2X] 38.304 corrections (CATT for discussion and 38.304 CR, Vivo for 36.304 CR)

Discuss the need of changes proposed from R2-2006620 and R2-2007877, detailed wordings if CR is required, and prepare agreeable 38.304 CR in R2-2008356 and 36.304 CR in R2-2008357. Note cover-page should be well written (with reasonable impact analysis). CRs will be approved by email. Deadline is 9/3 10:00am (UTC).

The remainder of this document is organized to discuss the corrections from {R2-2006620 and R2-2007877} ‎as the following. The discussions are in Section 2 and the conclusions are summarized in Section 3.

# 2 Discussion

## 2.1 NR sidelink reception

The related proposal is available in the below table:

|  |  |  |
| --- | --- | --- |
| Company | Tdoc | Proposals |
| CATT | R2-2006620‎ |  “The UE shall not perform NR sidelink ~~communication~~transmission according to SL-V2X-PreconfigurationNR if the UE detects a cell providing NR sidelink configuration or inter-carrier NR sidelink configuration for the frequency UE is interested to perform NR sidelink communication on.”  |

Consideration on the case that UE performs both NR and V2X sidelink ‎reception under the cell only providing NR sidelink configuration or V2X ‎sidelink configuration, there is no interference problem. E.g. if the UE ‎camps on a cell only providing V2X sidelink configuration and detects ‎another cell only providing NR sidelink configuration, the UE can ‎perform NR sidelink reception using pre-configuration. The UE is ‎unnecessary to reselect to the cell providing NR sidelink configuration to ‎perform NR sidelink reception. From the point of view of simplifying the ‎reception UE behaviour, the UE should be able to perform NR sidelink ‎reception according to SL-V2X-PreconfigurationNR even if the UE ‎detects a cell providing NR sidelink configuration or inter-carrier NR ‎sidelink configuration for the frequency that UE is interested to perform NR ‎sidelink communication on.‎ Thus, the CR in R2-2006620‎ proposed to change “NR sidelink communication” into “NR sidelink transmission” to simplify the ‎reception UE behaviour. Companies are encouraged to provide inputs on the following questions.

**Question1: Does company agree the 1st change in R2-2006620‎, i.e., change ‎“NR sidelink communication” into “NR sidelink transmission” in 38.304 as proposed in the above table?**

|  |  |  |
| --- | --- | --- |
| Company Name | Views: Agree/Disagree | Comments |
| Samsung | Disagree | We prefer to keep previous agreement not to use pre-configuration if the UE is in-coverage. RX operation has no problem without this enhancement. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

If the reason of 1st change in Q1 is an issue, Rapporteur ‎thinks we can further discuss whether it is necessary to make the similar change in 36.304, as below:

*The UE shall not perform V2X sidelink ~~communication~~transmission according to SL-V2X-Preconfiguration if the UE detects a cell providing V2X sidelink configuration or inter-carrier V2X sidelink configuration for the frequency UE is interested to perform V2X sidelink communication on.*

**Question2: Does company agree to make the change as above in 36.304?**

|  |  |  |
| --- | --- | --- |
| Company Name | Views: Agree/Disagree | Comments |
| Samsung | Disagree | Same as Q1. We prefer to keep previous agreement. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Proposed conclusion:**

TBD

## 2.2 RRC\_INACTIVE state

The related proposal is available in the below table:

|  |  |  |
| --- | --- | --- |
| Company | Tdoc | Proposals |
| CATT | R2-2006620‎ | ‎Add RRC\_INACTIVE state in cell selection and reselection for sidelink ‎operation in 38.304.The requirements defined in this clause for sidelink operation apply for UEs in RRC\_IDLE, RRC\_INACTIVE and in RRC\_CONNECTED. |
| vivo | R2-2007877‎ | Add RRC\_INACTIVE state in cell selection and reselection for sidelink ‎operation in 36.304.The requirements defined in this clause for sidelink operation apply for UEs in RRC\_IDLE, RRC\_INACTIVE and in RRC\_CONNECTED. |

RAN2 agreed to support a sidelink UE in all RRC states/coverage scenarios ‎‎(i.e. RRC\_CONNECTED, RRC\_INACTIVE/RRC\_IDLE, and OOC). However, ‎description of RRC\_INACTIVE is missing in cell (re)selection requirements ‎defined for sidelink operation. ‎Thus, the CR in R2-2006620‎ proposed to add RRC\_INACTIVE state in cell selection and reselection for ‎sidelink ‎operation in 38.304. The CR in R2-2006620‎ proposed to add RRC\_INACTIVE state also in 36.304. Companies are encouraged to provide inputs on the following question.

**Question3: Which option does company agree for RRC\_INACTIVE state in cell selection and reselection in sidelink ‎operation?‎**

**‎-‎ Option 1: Only add RRC\_INACTIVE state in ‎‎38.304‎, Clause 8.2;**

**‎-‎ Option 2: Only add RRC\_INACTIVE state in ‎‎36.304, Clause 11.4‎;**

**-‎ Option 3: Add RRC\_INACTIVE state in both 38.304, Clause 8.2 and 36.304, Clause 11.4;**

**- Option 4: Disagree to add RRC\_INACTIVE state in both 38.304 and 36.304.**

|  |  |  |
| --- | --- | --- |
| Company Name | Views: Option1/2/3/4 | Comments |
| Samsung | Option 3 |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Proposed conclusion:**

TBD

## 2.3 RRC\_INACTIVE state

The related proposal is available in the below table:

|  |  |  |
| --- | --- | --- |
| Company | Tdoc | Proposals |
| CATT | R2-2006620‎ | ‎When UE is interested to perform NR sidelink communication on non-serving frequency, it may perform measurements on that frequency or the frequencies which can provide inter carrier NR sidelink configuration for that frequency for cell selection and reselection purpose in accordance with TS 38.133[8]. When UE is interested to perform V2X sidelink communication on non-serving frequency, it may perform measurements on that frequency or the frequencies which can provide inter carrier V2X sidelink configuration for that frequency for cell selection and reselection purpose in accordance with TS 38.133[8]. |

Consideration on the case that UE performs both NR and V2X sidelink ‎communication under the cell only providing NR sidelink configuration or ‎V2X sidelink configuration, it can’t restrict UE to only perform intra-‎frequency cell reselection when UE is interested to perform NR sidelink ‎communication or V2X sidelink communication on non-serving ‎frequency. The UE shall perform inter-frequency or inter-RAT cell ‎reselection in this case.‎ Thus, the CR in R2-2006620‎ proposed to remove intra-frequency restriction for cell reselection when UE is ‎interested to perform NR sidelink ‎communication or V2X sidelink ‎communication on non-serving frequency.‎ Companies are encouraged to provide inputs on the following questions.

**Question4: Does company agree to remove intra-frequency restriction for cell reselection when UE is ‎interested to perform NR sidelink ‎communication ‎or V2X sidelink ‎communication on non-serving frequency‎ in 38.304?**

|  |  |  |
| --- | --- | --- |
| Company Name | Views: Agree/Disagree | Comments |
| Samsung | Agree |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

If the reason of Q4 is an issue, Rapporteur ‎thinks we can further discuss whether it is necessary to make the similar change in 36.304, as below:

*When UE is interested to perform sidelink communication or sidelink discovery announcement on non-serving frequency, it shall perform measurements on that frequency for cell selection and intra-frequency reselection purpose in accordance with TS 36.133 [10]. When UE is interested to perform V2X sidelink communication on non-serving frequency, it may perform measurements on that frequency or the frequencies which can provide inter-carrier V2X sidelink configuration for that frequency for cell selection and reselection purpose in accordance with TS 36.133 [10]. When UE is interested to perform NR sidelink communication on non-serving frequency, it may perform measurements on that frequency or the frequencies which can provide inter-carrier NR sidelink configuration for that frequency for cell selection and reselection purpose in accordance with TS 36.133[10].*

**Question5: Does company agree to remove intra-frequency restriction for cell reselection as above in 36.304?**

|  |  |  |
| --- | --- | --- |
| Company Name | Views: Agree/Disagree | Comments |
| Samsung | Agree |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Proposed conclusion:**

TBD

# 3 Conclusion

TBD

# 4 References

[1] RAN2-111-e\_V2X\_Kyeongin\_2020-08-28\_EOM