**3GPP TSG-RAN WG2 Meeting #113 Electronic *R2-210xxxx***

**Elbonia, 25 January – 05 February 2021**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.1* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  |  | **CR** |  | **rev** |  | **Current version:** | **15.12.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **x** | Radio Access Network | **x** | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Option 1: Clarification on the *supportedBandwidthCombinationSetIntraENDC* capability | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Nokia, Nokia Shanghai Bell | | | | | | | | | |
| ***Source to TSG:*** | R2 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | NR\_newRAT-Core | | | | |  | ***Date:*** | | | 2021-02-25 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **F** |  | | | | | ***Release:*** | | | 15 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-15 (Release 15) Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | It is unclear how the network knows the BCS given by the capability supportedBandwidthCombinationSetIntraENDC if a UE supports a combination that has an intra-band EN-DC component and the UE does not report an intra-band EN-DC BCS. Based on the incoming LS from RAN4 in R4-2103401 it is clarified in the RAN4 specifications that the intra-band configurations and BCSs apply to higher order EN-DC combinations with intra-band EN-DC only in the downlink and the default BCS is BCS0 for intra-band combinations. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | The capability *supportedBandwidthCombinationSetIntraENDC* is made optional with a default BCS0 assumption as guided by the RAN4 specifications.  **Impact analysis**  Impacted functionality: BCS reporting for intra-band EN-DC.  Impacted architecture options: (NG)EN-DC, NE-DC  Inter-operability:   1. If the network is implemented according to the CR and the UE is not, there are no inter-operability issues. 2. If the UE is implemented according to the CR and the network is not, there is no way for the network to know what is the default BCS that must be used for the intra-band EN-DC part in the downlink. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | It is unclear what the default BCS value the network must assume if the band combination is an intra-band (NG)EN-DC/NE-DC combination without supporting UL in both the bands of the intra-band (NG)EN-DC/NE-DC UL part. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 4.2.7.1 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  |  | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  |  | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  |  | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

*Modified Subclause*

4.2.7.1 *BandCombinationList* parameters

| **Definitions for parameters** | **Per** | **M** | **FDD-TDD**  **DIFF** | **FR1-FR2**  **DIFF** |
| --- | --- | --- | --- | --- |
| ***bandEUTRA***  Defines supported EUTRA frequency band by NR frequency band number, as specified in TS 36.101 [14]. | Band | Yes | N/A | N/A |
| ***bandList***  Each entry of the list should include at least one bandwidth class for UL or DL. | BC | Yes | N/A | N/A |
| ***bandNR***  Defines supported NR frequency band by NR frequency band number, as specified in TS 38.101-1 [2] and TS 38.101-2 [3]. | Band | Yes | N/A | N/A |
| ***ca-BandwidthClassDL-EUTRA***  Defines for DL, the class defined by the aggregated transmission bandwidth configuration and maximum number of component carriers supported by the UE, as specified in TS 36.101 [14]. When all FeatureSetEUTRA-DownlinkId:s in the corresponding FeatureSetsPerBand are zero, this field is absent. | Band | No | N/A | N/A |
| ***ca-BandwidthClassDL-NR***  Defines for DL, the class defined by the aggregated transmission bandwidth configuration and maximum number of component carriers supported by the UE, as specified in TS 38.101-1 [2] and TS 38.101-2 [3]. When all FeatureSetDownlinkId:s in the corresponding FeatureSetsPerBand are zero, this field is absent. For FR1, the value 'F' shall not be used as it is invalidated in TS 38.101-1 [2]. | Band | No | N/A | N/A |
| ***ca-BandwidthClassUL-EUTRA***  Defines for UL, the class defined by the aggregated transmission bandwidth configuration and maximum number of component carriers supported by the UE, as specified in TS 36.101 [14]. When all FeatureSetEUTRA-UplinkId:s in the corresponding FeatureSetsPerBand are zero, this field is absent. | Band | No | N/A | N/A |
| ***ca-BandwidthClassUL-NR***  Defines for UL, the class defined by the aggregated transmission bandwidth configuration and maximum number of component carriers supported by the UE, as specified in TS 38.101-1 [2] and TS 38.101-2 [3]. When all FeatureSetUplinkId:s in the corresponding FeatureSetsPerBand are zero, this field is absent. For FR1, the value 'F' shall not be used as it is invalidated in TS 38.101-1 [2]. | Band | No | N/A | N/A |
| ***ca-ParametersEUTRA***  Contains the EUTRA part of band combination parameters for a given (NG)EN-DC/NE-DC band combination. | BC | No | N/A | N/A |
| ***ca-ParametersNR***  Contains the NR band combination parameters for a given (NG)EN-DC/NE-DC and/or NR CA band combination. | BC | No | N/A | N/A |
| ***ca-ParametersNRDC***  Indicates whether the UE supports NR-DC for the band combination. It contains the NR band combination parameters applicable across MCG and SCG. In this version of the standard, a UE indicating support for NR-DC supports only configuration where all serving cells of the MCG are in FR1 and all serving cells of the SCG are in FR2. | BC | No | N/A | N/A |
| ***featureSetCombination***  Indicates the feature set that the UE supports on the NR and/or MR-DC band combination by FeatureSetCombinationId. | BC | N/A | N/ANo | N/A |
| ***mrdc-Parameters***  Contains the band combination parameters for a given (NG)EN-DC/NE-DC band combination. | BC | No | N/A | N/A |
| ***ne-DC-BC***  Indicates whether the UE supports NE-DC for the band combination. | BC | No | N/A | N/A |
| ***powerClass***  Indicates power class the UE supports when operating according to this band combination. If the field is absent, the UE supports the default power class. If this power class is higher than the power class that the UE supports on the individual bands of this band combination (*ue-PowerClass* in *BandNR*), the latter determines maximum TX power available in each band. The UE sets the power class parameter only in band combinations that are applicable as specified in TS 38.101-1 [2] and TS 38.101-3 [4]. | BC | No | N/A | FR1 only |
| ***SRS-SwitchingTimeNR***  Indicates the interruption time on DL/UL reception within a NR band pair during the RF retuning for switching between a carrier on one band and another (PUSCH-less) carrier on the other band to transmit SRS. *switchingTimeDL/ switchingTimeUL*:n0us represents 0 us, n30us represents 30us, and so on. *switchingTimeDL/ switchingTimeUL* is mandatory present if switching between the NR band pair is supported, otherwise the field is absent. It is signalled per pair of bands per band combination. | FD | No | N/A | N/A |
| ***SRS-SwitchingTimeEUTRA***  Indicates the interruption time on DL/UL reception within a EUTRA band pair during the RF retuning for switching between a carrier on one band and another (PUSCH-less) carrier on the other band to transmit SRS. *switchingTimeDL/ switchingTimeUL:* n0 represents 0 OFDM symbols, n0dot5 represents 0.5 OFDM symbols, n1 represents 1 OFDM symbol and so on. *switchingTimeDL/ switchingTimeUL* is mandatory present if switching between the EUTRA band pair is supported, otherwise the field is absent. It is signalled per pair of bands per band combination. | FD | No | N/A | N/A |
| ***srs-TxSwitch***  Defines whether UE supports SRS for DL CSI acquisition as defined in clause 6.2.1.2 of TS 38.214 [12]. The capability signalling comprises of the following parameters:  - *supportedSRS-TxPortSwitch* indicates SRS Tx port switching pattern supported by the UE. The indicated UE antenna switching capability of ′xTyR′ corresponds to a UE, capable of SRS transmission on ′x′ antenna ports over total of ′y′ antennas, where ′y′ corresponds to all or subset of UE receive antennas, where 2T4R is two pairs of antennas;  - *txSwitchImpactToRx* indicates the entry number of the first-listed band with UL (see NOTE) in the band combination that affects this DL;  - *txSwitchWithAnotherBand* indicates the entry number of the first-listed band with UL (see NOTE) in the band combination that switches together with this UL.  For *txSwitchImpactToRx* and *txSwitchWithAnotherBand*, value 1 means first entry, value 2 means second entry and so on. All DL and UL that switch together indicate the same entry number.  The entry number is the band entry number in a band combination. The UE is restricted not to include fallback band combinations for the purpose of indicating different SRS antenna switching capabilities.  NOTE: The first-listed band with UL includes a band associated with *FeatureSetUplinkId* set to 0 corresponding to the support of *SRS-SwitchingTimeNR*. | BC | Yes | N/A | N/A |
| ***supportedBandwidthCombinationSet***  Defines the supported bandwidth combination for the band combination set as defined in the TS 38.101-1 [2], TS 38.101-2 [3] and TS 38.101-3 [4]. For NR SA CA, NR-DC, inter-band (NG)EN-DC without intra-band (NG)EN-DC component, inter-band NE-DC without intra-band NE-DC component and intra-band (NG)EN-DC/NE-DC with additional inter-band NR CA component, the field defines the bandwidth combinations for the NR part of the band combination. For intra-band (NG)EN-DC/NE-DC without additional inter-band NR and LTE CA component, the field indicates the supported bandwidth combination set applicable to the NR and LTE band combinations. Field encoded as a bit map, where bit N is set to "1" if UE support Bandwidth Combination Set N for this band combination as defined in the TS 38.101-1 [2], TS 38.101-2 [3] and TS 38.101-3 [4]. The leading / leftmost bit (bit 0) corresponds to the Bandwidth Combination Set 0, the next bit corresponds to the Bandwidth Combination Set 1 and so on. It is mandatory if the band combination has more than one NR carrier (at least one SCell in an NR cell group) or is an intra-band (NG)EN-DC/NE-DC combination or both. | BC | CY | N/A | N/A |
| ***supportedBandwidthCombinationSetIntraENDC***  Defines the supported bandwidth combination for the band combination set as defined in the TS 38.101-3 [4]. For intra-band (NG)EN-DC with additional inter-band CA component(s) of LTE and/or NR, the field defines the bandwidth combinations for the intra-band (NG)EN-DC component. For intra-band NE-DC with additional inter-band CA component(s) of LTE and/or NR, the field defines the bandwidth combinations for the intra-band NE-DC component. Field encoded as a bit map, where bit N is set to "1" if UE support Bandwidth Combination Set N for this band combination as defined in the TS 38.101-3 [4]. The leading / leftmost bit (bit 0) corresponds to the Bandwidth Combination Set 0, the next bit corresponds to the Bandwidth Combination Set 1 and so on.   * It is mandatory if the band combination is an intra-band (NG)EN-DC/NE-DC combination supporting both UL and DL intra-band (NG)EN-DC/NE-DC parts as defined in TS 38.101-3 [4] with additional inter-band NR/LTE CA component. * It is optional if the band combination is an intra-band (NG)EN-DC/NE-DC combination without supporting UL in both the bands of the intra-band (NG)EN-DC/NE-DC UL part as defined in TS 38.101-3 [4]. In this case BCS0 is the default value for DL part of the intra-band (NG)EN-DC/NE-DC. | BC | CY | N/A | N/A |

*End of Changes*