**3GPP TSG-RAN WG2 #113bis-e *R2-210xxxx***

**E-meeting, April 2021**

Agenda Item: 8.15.2.1

Source: OPPO

Title: Summary of [POST113-e][704][V2X/SL] TX UE centric or RX UE centric DRX configuration determination (OPPO)

Document for: Discussion, Decision

# Introduction

This is for the following email discussion

**[POST113-e][704][V2X/SL] TX UE centric or RX UE centric DRX configuration determination (OPPO)**

**Scope:** Continue the discussion the remained issues regarding who will determine DRX configurations (including TX UE centric vs RX UE centric DRX configuration determination), covering both in and out of coverage scenario.

**Intended outcome:** Discussion summary

**Deadline:** Long email discussion

# Discussion

## For OOC scenario

In this email discussion, we will limit to unicast case.

Base on online discussion at RAN2#113

4: For unicast, for OOC scenario, the UE who sends out the DRX configuration decides on the DRX configuration. FFS on whether pre-configuration and/or the assistance information from the peer UE is also taken into account when determining the DRX configuration.

5: For unicast, for OOC scenario, adopt per-direction DRX configuration is as baseline. FFS on whether it is TX-centric or Rx-centric, i.e. TX UE or RX UE decides it.

As discussed in R2-2102183, the per-direction DRX configuration is something as follows:

*But to look into the core issue, rapporteur suggest the following simplification for the scenario:*

* *Start from OOC scenario to avoid the discussion on gNB involvement as a start point;*
* *Do not touch the failure handling or the negotiation procedure (i.e., in case the DRX configuration is not preferred by the peer UE) in this discussion;*
* *Do not touch the assistance information (information from peer UE to assist the DRX configuration decision) in this discussion;*

*Based on the assumption above, firstly we can look at the options on the table.*

***Option-A: Per-direction DRX configuration***

*Option-A1: Per-direction DRX configuration + Tx-centric manner, i.e., it is the Tx-UE who decide the DRX configuration of Rx-UE, and send it to Rx-UE.*

*NOTE: in the figure below, the timing for UE1/2 send out the configuration is not restricted.*

**

*Figure 1 Per-direction DRX configuration + Tx-centric manner*

*Option-A2: Per-direction DRX configuration + Rx-centric manner, i.e., it is the Rx-UE who decide the DRX configuration of Rx-UE, and send it to Tx-UE.*

*NOTE: in the figure below, the timing for UE1/2 send out the configuration is not restricted.*

**

*Figure 2 Per-direction DRX configuration + Rx-centric manner*

**NOTE: In the following, the discussion is for a single direction, i.e., UE1 as TX-UE and UE2 as RX-UE. The other direction is not shown in the figure by assuming a symmetric procedure is applied to UE2 as TX-UE and UE1 as RX-UE.**

On the one hand, based on the discussion in RAN2#113, rapporteur understand there is no clear majority on either TX or RX centric manner.

* TX-centric: UE1 send out the DRX configuration to UE2 for UE1=>UE2 direction;
* Rx-centric: UE2 send out the DRX configuration to UE1 for UE1=>UE2 direction;

On the other hand, for each option, there are companies proposing assistance information from the counterpart UE, to avoid unilateral decision, which (assistance information) is in the scope of RAN2#113 discussion in R2-2102183.

|  |  |  |
| --- | --- | --- |
| InterDigital | Yes | […]To the above options, we should add:* **Option A3**: Per direction DRX configuration, TX centric, using information from the RX UE. Here, the TX UE first receives information from the RX UE, decides the DRX configuration for the RX UE based on the information provided, and sends the DRX configuration to the RX UE.
* **Option A4:** Per direction DRX configuration, RX centric, using information from the TX UE. Here the RX UE first receives information from the TX UE, decides its DRX configuration from the received information, and sends its DRX configuration to the TX UE.

[…]  |

* Assistance information for TX-centric: UE2 send out the DRX configuration to UE1 for UE1=>UE2 direction;
* Assistance information for RX-centric: UE1 send out the DRX configuration to UE2 for UE1=>UE2 direction;

So rapporteur suggests we ignore the form of signalling for a while, and if merge

* The two as signalling from UE2 as RX-UE on the DRX configuration;
* The two as signalling from UE1 as TX-UE on the DRX configuration;

**Q1: For the direction of UE1 as Tx-UE and UE2 as Rx-UE, if define**

* **Signaling-1: As signalling from UE2 (RX-UE) to UE1 (TX-UE) including the DRX configuration;**
* **Signaling-2: As signalling from UE1 (TX-UE) to UE2 (RX-UE) including the DRX configuration;**

**which signalling should be supported (regardless of the signalling form, e.g., as configuration, or as assistance information or etc.)**

**Option-1: Both signalling-1 and signalling-2;**

**Option-2: Signalling-1 only;**

**Option-3: Signalling-2 only;**

|  |  |  |
| --- | --- | --- |
| Company | Option | Comment |
| OPPO | Option-1 or Option-3 | Considering the legacy signalling framework on PC5, signalling from Tx-UE to Rx-UE for the configuration of direction from Tx-UE to Rx-UE is necessary.While the assistance signalling from Rx-UE to Tx-UE can be used additionally to take preference from Rx-UE into account. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

Then the next question is in which form the signalling-1/2 is to be delivered, possible signalling includes:

Option-A: Using *RRCReconfigurationSidelink;*

Option-B: Using *RRCReconfigurationFailureSidelink*, e.g., this message is used to suggest a DRX configuration that is different from the one included in *RRCReconfigurationSidelink*;

Option-C: Using a new PC5-RRC message, e.g., one can mimic the UAI message as used in Uu-RRC;

**Q2a: If one answer option-1 and/or option-2 for Q1, i.e., agree the necessity of signaling-1 (i.e., signalling from UE2 (RX-UE) to UE1 (TX-UE) including the DRX configuration), which PC5-RRC message can be used to carry signaling-1?**

**Option-A: Using *RRCReconfigurationSidelink;***

**Option-B: Using *RRCReconfigurationFailureSidelink*, e.g., this message is used to suggest a DRX configuration that is different from the one included in *RRCReconfigurationSidelink*;**

**Option-C: Using a new PC5-RRC message, e.g., one can mimic the UAI message as used in Uu-RRC;**

**Option-D: Other**

|  |  |  |
| --- | --- | --- |
| Company | Option | Comment |
| OPPO | Option-B or Option-C | Comparing the two approaches, i.e., TX-centric and RX-centric

|  |  |  |
| --- | --- | --- |
| Disadvantage | If rely on Rx-UE to control the DRX configuration | If rely on Tx-UE to control the DRX configuration |
| 1 | Two RX-UE may require a TX-UE to send data on the same resource, but that is infeasible since TX-UE can only perform one single transmission at one slot. | different TX-UE may require a same RX-UE to wake up at different time, so increase the power consumption. |
| 2 | It violates the sidelink design framework of “Tx-centric” since Rel-12, i.e., Tx-UE itself (or the network behind) to decide on the transmission. In more details, the Rx-UE has no information on Tx-side traffic characteristics and resource configuration. Signaling-wise, currently PC5-RRC design is to rely on TX-UE to configure SDAP/PDCP/RLC/MAC/PHY configuration. If DRX configuration becomes an exceptional case, i.e., only this parameter is configured by Rx-UE, then when there is any causality / coupling between DRX and other parameters, it becomes a chicken-and-egg issue, i.e., two related parameters configured by two separate entities (i.e., TX-UE and RX-UE), which may further cause discussion / work on how to coordinate between the two entities |  |
| 3 | Without information of Tx-side traffic characteristics and resource configuration, it is not feasible to rely on Rx-UE to make a final decision on the DRX configuration  |  |

I.e., it seems TX-centric approach have more (less) advantages (disadvantages), especially considering that the only disadvantage can be alleviated by assistance information from RX-UE.For option-B, it allows the Rx-UE to decide on a DRX configuration which is different from the one sent by Tx-UE configuration. For option-C, it allows the Rx-UE to suggest a DRX configuration before the Tx-UE sending a DRX configuration. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Q2b: If one answer option-1 and/or option-3 for Q1, i.e., agree the necessity of signaling-2 (i.e., signalling from UE1 (TX-UE) to UE2 (RX-UE) including the DRX configuration), which PC5-RRC message can be used to carry signaling-2?**

**Option-A: Using *RRCReconfigurationSidelink;***

**Option-B: Using *RRCReconfigurationFailureSidelink*, e.g., this message is used to suggest a DRX configuration that is different from the one included in *RRCReconfigurationSidelink*;**

**Option-C: Using a new PC5-RRC message, e.g., one can mimic the UAI message as used in Uu-RRC;**

**Option-D: Other**

|  |  |  |
| --- | --- | --- |
| Company | Option | Comment |
| OPPO | Option-A | Comparing the two approaches, i.e., TX-centric and RX-centric

|  |  |  |
| --- | --- | --- |
| Disadvantage | If rely on Rx-UE to control the DRX configuration | If rely on Tx-UE to control the DRX configuration |
| 1 | Two RX-UE may require a TX-UE to send data on the same resource, but that is infeasible since TX-UE can only perform one single transmission at one slot. | different TX-UE may require a same RX-UE to wake up at different time, so increase the power consumption. |
| 2 | It violates the sidelink design framework of “Tx-centric” since Rel-12, i.e., Tx-UE itself (or the network behind) to decide on the transmission. In more details, the Rx-UE has no information on Tx-side traffic characteristics and resource configuration. Signaling-wise, currently PC5-RRC design is to rely on TX-UE to configure SDAP/PDCP/RLC/MAC/PHY configuration. If DRX configuration becomes an exceptional case, i.e., only this parameter is configured by Rx-UE, then when there is any causality / coupling between DRX and other parameters, it becomes a chicken-and-egg issue, i.e., two related parameters configured by two separate entities (i.e., TX-UE and RX-UE), which may further cause discussion / work on how to coordinate between the two entities |  |
| 3 | Without information of Tx-side traffic characteristics and resource configuration, it is not feasible to rely on Rx-UE to make a final decision on the DRX configuration  |  |

I.e., it seems TX-centric approach have more (less) advantages (disadvantages), especially considering that the only disadvantage can be alleviated by assistance information from RX-UE.By using option-A, it allows a simple two step configuration as the very basic procedure, i.e., *RRCReconfigurationSidelink* + *RRCReconfigurationCompleteSidelink* (in case the DRX configuration is acceptable to Rx-UE). |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

Then the third question is how for the UE to derive the DRX configuration that is to be included in the signaling, which is the continuation of the agreement from RAN2#113 as follows

4: For unicast, for OOC scenario, the UE who sends out the DRX configuration decides on the DRX configuration. FFS on whether pre-configuration and/or the assistance information from the peer UE is also taken into account when determining the DRX configuration.

**By assuming the questions (Q1 and Q2a/b) above have already covered the FFS point on assistance information**, the only left FFS is on pre-configuration, i.e., whether it is has to be taken into account or not.

**Q3a: If one answer option-1 and/or option-2 for Q1, i.e., agree the necessity of signaling-1 (i.e., signalling from UE2 (RX-UE) to UE1 (TX-UE) including the DRX configuration), in case of OOC scenario, how for UE2 to derive the DRX configuration that is to be included in signaling-1 (assuming the necessity of assistance information has been covered by Q1/Q2a/Q2b)?**

**Option-A: Decided by UE implementation without relying pre-configuration*;***

**Option-B: Decided by UE implementation taking into account of input from pre-configuration;**

|  |  |  |
| --- | --- | --- |
| Company | Option | Comment |
| OPPO | Option-A | In practice, pre-configuration can only achieve common configuration between UEs (no matter it is one or multiple DRX configuration), which is not aligned with the design spirit of unicast DRX configuration, i.e., per-direction DRX configuration. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Q3b: If one answer option-1 and/or option-2 for Q1, i.e., agree the necessity of signaling-2 (i.e., signalling from UE1 (TX-UE) to UE2 (RX-UE) including the DRX configuration), in case of OOC scenario, how for UE1 to derive the DRX configuration that is to be included in signaling-1 (assuming the necessity of assistance information has been covered by Q1/Q2a/Q2b)?**

**Option-A: Decided by UE implementation without relying pre-configuration*;***

**Option-B: Decided by UE implementation taking into account of input from pre-configuration;**

|  |  |  |
| --- | --- | --- |
| Company | Option | Comment |
| OPPO | Option-A | In practice, pre-configuration can only achieve common configuration between UEs (no matter it is one or multiple DRX configuration), which is not aligned with the design spirit of unicast DRX configuration, i.e., per-direction DRX configuration. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

## For IC scenario

For in-coverage scenario, RAN may be involved in the whole procedure, e.g., for a signalling-X from UE-A to UE-B (Please note that UE-A can be either UE-1 or UE-2, i.e., either TX-UE or RX-UE, and similarly for UE-B. The questions below has clarified the applied UE explicitly),

* The first question is how for the UE-A to generate the signalling, taking into account of SIB/dedicated-RRC or not;
* The second question is whether the UE-B needs to reflect the signalling to network using dedicated-RRC or not;



**Q4a: If one answer option-1 and/or option-2 for Q1, i.e., agree the necessity of signaling-1 (i.e., signalling from UE2 (RX-UE) to UE1 (TX-UE) including the DRX configuration), If UE-2 is in-coverage, in RRC\_IDLE/RRC\_INACTIVE state, how for UE2 to derive the DRX configuration that is to be included in signaling-1?**

**Option-A: Decided by UE implementation without relying SIB*;***

**Option-B: Decided by UE implementation taking into account of input from SIB;**

|  |  |  |
| --- | --- | --- |
| Company | Option | Comment |
| OPPO | Option-A | Same logic as for pre-configuration, i.e., SIB cannot achieve per-UE configuration, so no need to take into account. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Q4b: If one answer option-1 and/or option-2 for Q1, i.e., agree the necessity of signaling-1 (i.e., signalling from UE2 (RX-UE) to UE1 (TX-UE) including the DRX configuration), If UE-2 is in-coverage, in RRC\_CONNECTED state, how for UE2 to derive the DRX configuration that is to be included in signaling-1?**

**Option-A: Decided by UE implementation without relying dedicated RRC or SIB*;***

**Option-B: Decided by UE implementation taking into account of input from SIB;**

**Option-C: Decided by UE implementation taking into account of input from dedicated RRC;**

|  |  |  |
| --- | --- | --- |
| Company | Option | Comment |
| OPPO | Option-A or Option-C | Same logic as for pre-configuration, i.e., SIB cannot achieve per-UE configuration, so no need to take into account. While dedicated-RRC may help the network to take it into control. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Q4c: If one answer option-1 and/or option-2 for Q1, i.e., agree the necessity of signaling-1 (i.e., signalling from UE2 (RX-UE) to UE1 (TX-UE) including the DRX configuration), if UE-1 is in-coverage, in RRC\_CONNECTED state, whether UE-1 needs to report the DRX configuration received in signaling-1 to the serving network?**

|  |  |  |
| --- | --- | --- |
| Company | Yes/No | Comment |
| OPPO | Yes | As answered for Q5b, since the dedicated-RRC is necessary for network to take DRX configuration into control, the report of signalling-1 is also useful. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Q5a: If one answer option-1 and/or option-3 for Q1, i.e., agree the necessity of signaling-2 (i.e., signalling from UE1 (TX-UE) to UE2 (RX-UE) including the DRX configuration), If UE-1 is in-coverage, in RRC\_IDLE/RRC\_INACTIVE state, how for UE1 to derive the DRX configuration that is to be included in signaling-2?**

**Option-A: Decided by UE implementation without relying SIB*;***

**Option-B: Decided by UE implementation taking into account of input from SIB;**

|  |  |  |
| --- | --- | --- |
| Company | Option | Comment |
| OPPO | Option-A |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Q5b: If one answer option-1 and/or option-3 for Q1, i.e., agree the necessity of signaling-2 (i.e., signalling from UE1 (TX-UE) to UE2 (RX-UE) including the DRX configuration), If UE-1 is in-coverage, in RRC\_CONNECTED state, how for UE1 to derive the DRX configuration that is to be included in signaling-2?**

**Option-A: Decided by UE implementation without relying dedicated RRC or SIB*;***

**Option-B: Decided by UE implementation taking into account of input from SIB;**

**Option-C: Decided by UE implementation taking into account of input from dedicated RRC;**

|  |  |  |
| --- | --- | --- |
| Company | Option | Comment |
| OPPO | Option-C | Dedicated-RRC is necessary to take DRX configuration into network control.Same logic as for pre-configuration, i.e., SIB cannot achieve per-UE configuration, so no need to take into account.  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Q5c: If one answer option-1 and/or option-3 for Q1, i.e., agree the necessity of signaling-2 (i.e., signalling from UE1 (TX-UE) to UE2 (RX-UE) including the DRX configuration), If UE-2 is in-coverage, in RRC\_CONNECTED state, whether UE-2 needs to report the DRX configuration received in signaling-2 to the serving network?**

|  |  |  |
| --- | --- | --- |
| Company | Yes/No | Comment |
| OPPO | Yes | It is necessary for UE2 network to take into account the SL DRX configuration when deciding the Uu DRX configuration. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

1. xxx.

# Conclusion

We have the following proposals

[Proposal 1 xxx.](#_Toc62216175)

# Reference