3GPP TSG-RAN WG2#113-bis-e DocNumber

Electronic meeting, 12th April – 20th April 2021

Agenda Item: 6.10.1

Source: Ericsson

Title: Report of email discussion on Timestamp of event triggered MDT

Document for: Discussion, Decision

# 1 Introduction

This contribution is related to the following email discussion.

* [Post113-e][NR/R16 SON/MDT]  Timestamp of event triggered MDT (Ericsson)

- Focus on the issue “Timestamp of event triggered logged MDT” in R2-2102141.

- Figure out the UE behaviour

Intended outcome: Report

Deadline: Next meeting

The intention of this email discussion is to identify the intended UE behavior for the when the UE includes measurements in the event triggered logging of measurements in the logged MDT procedure.

The email discussion will be in two phases. During the first phase, the email discussion will be using the questionnaire in this contribution. In the second phase, companies can check the summary of the outcome of the email discussion (the deadlines are as per the chairman’s guideline wherein March 29th to April 5th is classified as silent period).

Phase-1:

Intended outcome: Identification of the UEs expected behaviour for event triggered logged MDT (if any)

Deadline: Wednesday 24/03/2021 23:59 UTC

Phase-2:

Intended outcome: agree on the summary and TP (if any)

Deadline: Friday 26/03/2021 23:59 UTC

# 2 Contact Information

|  |  |
| --- | --- |
| Company | Contact: Name (E-mail) |
| Ericsson | pradeepa.ramachandra@ericsson.com |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

# 3 Discussion

In the following, event-L1 is taken as an example for explaining the different understanding of companies.

## 3.1 Event L1 related

During the RAN2#113-e meeting, an offline discussion [1] was held on the topic of time stamp related information inclusion for the event triggered logged MDT. In this email discussion, companies expressed two different understanding of the specification text.

1. **Option-1A: Based on the field description of the event L1**
2. **Option-2A: Based on the procedural text of the event L1**

These options are better explained using the following figures.

L1 threshold

T1

T2

TTT

loggingInterval

T3

T4

Figure 1: Example scenario associated to the logging of measurements in L1 event based logged MDT

### Option-A1: Based on the field description of the event L1

Specification Reference (TS 38.331) for this option:

| ***eventType***  The value outOfCoverage indicates the UE to perform logging of measurements when the UE enters any cell selection state, and the value eventL1 indicates the UE to perform logging of measurements when the triggering condition (similar as event A2 as specified in 5.5.4.3) as configured in the event is met for the camping cell in camped normally state. |
| --- |

The UE logs measurements when the event entering conditions (threshold +TTT condition) are satisfied for the first time and then subsequently at every expiry of ‘*loggingInterval*’ if the event entering condition is satisfied (threshold condition). Based on this understanding of the specification, the UE logs as per Table 1.

|  |  |
| --- | --- |
| First instance of logging measurement | T2 |
| Second instance of logging measurement | T3 |
| Third instance of logging measurement | T4 |

Table 1: Logging of measurements as per option-A1 based understanding of the specification

As listed in the table, the UE logs the first measurement at time=T2 and then subsequently at every *loggingInterval* from that point in time (i.e., at T3, T4). This is as per the UE behaviour for event-A2 in RRC connected mode wherein the procedural text for first transmission of measurement report would trigger the start of periodical timer with the value *reportInterval* associated to the subsequent transmission of measurement report (excerpts from the section 5.5.5.1 is given below).

1> if the *numberOfReportsSent* as defined within the *VarMeasReportList* for this *measId* is less than the *reportAmount* as defined within the corresponding *reportConfig* for this *measId*:

2> start the periodical reporting timer with the value of *reportInterval* as defined within the corresponding *reportConfig* for this *measId*;

Thus, the option-A1 follows the UE behaviour inline with event-A2.

### Option-A2: Based on the procedural text of the event L1

Specification Reference (TS 38.331) for this option:

2> else if the *reportType* is set to *eventTriggered* and *eventType* is set to *eventL1*:

3> if the UE is in camped normally state on an NR cell and if the RPLMN is included in *plmn-IdentityList* stored in *VarLogMeasReport* and, if the cell is part of the area indicated by *areaConfiguration* if configured in *VarLogMeasConfig*;

4> perform the logging at regular time intervals as defined by the *loggingInterval* in *VarLogMeasConfig* only when the conditions indicated by the *eventL1* are met;

At every expiry of ‘*loggingInterval*’ if the event entering conditions are satisfied (threshold+TTT condition). Based on this understanding of the specification, the UE logs as per Table 2.

|  |  |
| --- | --- |
| First instance of logging measurement | T3 |
| Second instance of logging measurement | T4 |

Table 2: Logging of measurements as per option-A2 based understanding of the specification

As listed in the table, the UE logs the first measurement at time=T3 as this is the first time when the loggingInterval related criterion is fulfilled after meeting the event entering condition. Further on, the UE logs measurements subsequently at every *loggingInterval* from that point in time (i.e., at T4).

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

Based on this, the rapporteur would like to request companies to provide their views on what is their current understanding of the UE’s expected behaviour for L1 event.

**Question-1: Which of the following is the expected UE behavior for the event L1 based logging of measurements in logged MDT (please add any new option based on you understanding of the specification)?**

1. **Option-1A: Based on the field description of the event L1**
2. **Option-2A: Based on the procedural text of the event L1**
3. **Option-3A: ??**

|  |  |  |
| --- | --- | --- |
| **Company Name** | **Option-1A/Option-2A** | **Comments (if any changes are to be proposed, please include them here)** |
| Ericsson | Option-1A | As the intention of the event-L1 is to reflect the UE behavior of connected mode event-A2 for the idle/inactive UEs in terms of logging of measurements, we believe the option-1A is the correct solution.  With the option-2A, the network does not get the required information about when the poor coverage of the serving cell started (the time ‘T2’ in the scenario depicted in Figure 1). Further, there is a risk that the UE does not store any information about the event-L1 if the UE satisfies the event entering conditions (threshold+TTT) but before the first loggingInterval is expired, the event entering condition is no more satisfied. |
|  |  |  |
|  |  |  |

**Rapportuer summary**: To be added later

## 3.2 *OutOfCoverage* event related

The issue captured for the event L1 based event trigged logged MDT is also applicable for the out-of-coverage based event triggered logged MDT as the field description and the procedural text could cause the same interpretation issues explained for event L1. The corresponding figure illustrating this issue is shown in Figure 2. At time = T1, the UE fails to meet the s-criterion (suitability criterion) for any of the cells that are part of the cell reselection process and after 10 more seconds (section 4.2.2.2 in [2]), i.e., at T2, the UE enters the any cell selection state.

S-criterion Threshold

T1

T2

10 sec

loggingInterval

T3

T4

Figure 2: Example scenario associated to the logging of measurements in *outOfCoverage* based logged MDT

Two different understanding of the specification text for this scenario is given below.

1. **Option-1B: Based on the field description of the *outOfCoverage* event**
2. **Option-2B: Based on the procedural text of the *outOfCoverage* event**

### Option-1B: Based on the field description of the *outOfCoverage*

Field description associated to *outOfCoverage* event

| ***eventType***  The value outOfCoverage indicates the UE to perform logging of measurements when the UE enters any cell selection state, and the value eventL1 indicates the UE to perform logging of measurements when the triggering condition (similar as event A2 as specified in 5.5.4.3) as configured in the event is met for the camping cell in camped normally state. |
| --- |

Based on this understanding of the specification, the UE logs as per Table 3.

|  |  |
| --- | --- |
| First instance of logging measurement | T2 |
| Second instance of logging measurement | T3 |
| Third instance of logging measurement | T4 |

Table 3: Logging of measurements as per option-1B based understanding of the specification

### Option-2B: Based on the procedural text of the *outOfCoverage*

Procedural text associated to *outOfCoverage* event

2> else if the *reportType* is set to *eventTriggered*, and *eventType* is set to *outOfCoverage*:

3> perform the logging at regular time intervals as defined by the *loggingInterval* in *VarLogMeasConfig* only when the UE is in any cell selection state;

3> perform the logging immediately upon transitioning from the any cell selection state to the camped normally state;

Based on this understanding of the specification, the UE logs as per Table 4.

|  |  |
| --- | --- |
| First instance of logging measurement | T3 |
| Second instance of logging measurement | T4 |

Table 4: Logging of measurements as per option-2B based understanding of the specification

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

Based on this, the rapporteur would like to request companies to provide their views on what is their current understanding of the UE’s expected behaviour for *outOfCoverage* event.

**Question-2: Which of the following is the expected UE behavior for the *outOfCoverage* event based logging of measurements in logged MDT (please add any new option based on you understanding of the specification)?**

1. **Option-1B: Based on the field description of the outOfCoverage event**
2. **Option-2B: Based on the procedural text of the outOfCoverage event**
3. **Option-3B: ??**

|  |  |  |
| --- | --- | --- |
| **Company Name** | **Option-1B/Option-2B** | **Comments (if any changes are to be proposed, please include them here)** |
| Ericsson | Option-1B | Similar reasoning as previous question.  With the option-2B, the network does not get the required information about when the UE entered the any cell selection state (the time ‘T2’ in the scenario depicted in Figure 2). Further, there is a risk that the UE does not store any information about the outOfCoverage event if the UE satisfies the event entering conditions (enters any cell selection state) but before the first loggingInterval is expired, the UE returns to the camped normally state. |
|  |  |  |
|  |  |  |

**Rapportuer summary**: To be added later

## 3.3 Specification clarification

Associated to the issues listed in section 3.1 and section 3.2, the rapporteur believes that some corrections can be performed in the RRC specification to avoid any confusion in the future. Associated to this TPs are provided for option-1A+option-1B based understanding in section 5.1 and for option-2A+option-2B based understanding in section 5.2. Companies are requested to check if they are fine with the changes proposed in the TP or not.

**Question-3: Which of the following changes is agreeable?**

1. **Option-1: Changes as captured in section 5.1**
2. **Option-2: Changes as captured in section 5.2**
3. **Option-3: No changes.**

|  |  |  |
| --- | --- | --- |
| **Company Name** | **Option-1/Option-2/ Option-3** | **Comments (if any changes are to be proposed, please include them here)** |
| Ericsson | Option-1 | As the changes in section 5.1 captures the procedural text for the UE in a better way, we prefer to have this change included so as to avoid different UE implementations based on different interpretation of the specification. |
|  |  |  |
|  |  |  |

**Rapportuer summary**: To be added later

# 3 Conclusion

To be added later

# 4 References

1. R2-2102141, Report of [AT113-e][804][NR/R16 SON/MDT] Stage-2 corrections, CMCC, Nokia, RAN2#113-e meeting, Jan-Feb 2021.
2. TS 38.133

# 5 TP for TS 38.331

## 5.1 Option-1A and Option-1B based TP for TS 38.331

5.5a.3.2 Initiation

While T330 is running, the UE shall:

1> perform the logging in accordance with the following:

2> if the *reportType* is set to *periodical* in the *VarLogMeasConfig*:

3> if the UE is in camped normally state on an NR cell and if the RPLMN is included in *plmn-IdentityList* stored in *VarLogMeasReport:*

4> if areaConfiguration is not included in *VarLogMeasConfig*; or

4> if the serving cell is part of the area indicated by *areaConfig* in *areaConfiguration* in *VarLogMeasConfig*:

5> perform the logging at regular time intervals, as defined by the *loggingInterval* in the *VarLogMeasConfig*;

2> else if the *reportType* is set to *eventTriggered*, and *eventType* is set to *outOfCoverage*:

3> perform the logging upon entering the any cell selection state and from then on at regular time intervals as defined by the *loggingInterval* in *VarLogMeasConfig* only when the UE is in any cell selection state;

3> perform the logging immediately upon transitioning from the any cell selection state to the camped normally state;

2> else if the *reportType* is set to *eventTriggered* and *eventType* is set to *eventL1*:

3> if the UE is in camped normally state on an NR cell and if the RPLMN is included in *plmn-IdentityList* stored in *VarLogMeasReport:*

4> if *areaConfiguration* is not included in *VarLogMeasConfig*; or

4> if the serving cell is part of the area indicated by *areaConfig* in *areaConfiguration* in *VarLogMeasConfig*;

5> perform the logging upon satisfying the conditions indicated by the *eventL1* and from then on at regular time intervals as defined by the *loggingInterval* in *VarLogMeasConfig* only when the conditions indicated by the *eventL1* are met;

2> when performing the logging:

3> set the *relativeTimeStamp* to indicate the elapsed time since the moment at which the logged measurement configuration was received;

3> if detailed location information became available during the last logging interval, set the content of the *locationInfo* as in 5.3.3.7:

3> if the UE is in any cell selection state (as specified in TS 38.304 [20]):

4> set *anyCellSelectionDetected* to indicate the detection of no suitable or no acceptable cell found;

4> set the *servCellIdentity* to indicate global cell identity of the last logged cell that the UE was camping on;

4> set the *measResultServingCell* to include the quantities of the last logged cell the UE was camping on;

3> else:

4> set the *servCellIdentity* to indicate global cell identity of the cell the UE is camping on;

4> set the *measResultServingCell* to include the quantities of the cell the UE is camping on;

3> if available, set the *measResultNeighCells*, in order of decreasing ranking-criterion as used for cell re-selection, to include measurements of neighbouring cell that became available during the last logging interval and according to the following:

4> include measurement results for at most 6 neighbouring cells on the NR serving frequency and for at most 3 cells per NR neighbouring frequency and for the NR neighbouring frequencies in accordance with the following:

5> if *interFreqTargetInfo* is included in *VarLogMeasConfig*:

6> include measurement results for NR neighbouring frequencies that are included in both *interFreqTargetInfo* and *SIB4*;

5> else:

6> include measurement results for NR neighbouring frequencies that are included in *SIB4*;

4> include measurement results for at most 3 neighbours per inter-RAT frequency that is included in *SIB5*;

4> for each neighbour cell included, include the optional fields that are available;

NOTE: The UE includes the latest results of the available measurements as used for cell reselection evaluation in RRC\_IDLE or RRC\_INACTIVE, which are performed in accordance with the performance requirements as specified in TS 38.133 [14].

2> when the memory reserved for the logged measurement information becomes full, stop timer T330 and perform the same actions as performed upon expiry of T330, as specified in 5.5a.1.4.

## 5.2 Option-2A and Option-2B based TP for TS 38.331

### 6.2.2 Message definitions

– *LoggedMeasurementConfiguration*

The *LoggedMeasurementConfiguration* message is used to perform logging of measurement results while in RRC\_IDLE or RRC\_INACTIVE. It is used to transfer the logged measurement configuration for network performance optimisation.

Signalling radio bearer: SRB1

RLC-SAP: AM

Logical channel: DCCH

Direction: Network to UE

1. ***LoggedMeasurementConfiguration message***

-- ASN1START

-- TAG-LOGGEDMEASUREMENTCONFIGURATION-START

LoggedMeasurementConfiguration-r16 ::= SEQUENCE {

criticalExtensions CHOICE {

loggedMeasurementConfiguration-r16 LoggedMeasurementConfiguration-r16-IEs,

criticalExtensionsFuture SEQUENCE {}

}

}

LoggedMeasurementConfiguration-r16-IEs ::= SEQUENCE {

traceReference-r16 TraceReference-r16,

traceRecordingSessionRef-r16 OCTET STRING (SIZE (2)),

tce-Id-r16 OCTET STRING (SIZE (1)),

absoluteTimeInfo-r16 AbsoluteTimeInfo-r16,

areaConfiguration-r16 AreaConfiguration-r16 OPTIONAL, --Need R

plmn-IdentityList-r16 PLMN-IdentityList2-r16 OPTIONAL, --Need R

bt-NameList-r16 SetupRelease {BT-NameList-r16} OPTIONAL, --Need M

wlan-NameList-r16 SetupRelease {WLAN-NameList-r16} OPTIONAL, --Need M

sensor-NameList-r16 SetupRelease {Sensor-NameList-r16} OPTIONAL, --Need M

loggingDuration-r16 LoggingDuration-r16,

reportType CHOICE {

periodical LoggedPeriodicalReportConfig-r16,

eventTriggered LoggedEventTriggerConfig-r16,

...

},

lateNonCriticalExtension OCTET STRING OPTIONAL,

nonCriticalExtension SEQUENCE {} OPTIONAL

}

LoggedPeriodicalReportConfig-r16 ::= SEQUENCE {

loggingInterval-r16 LoggingInterval-r16,

...

}

LoggedEventTriggerConfig-r16 ::= SEQUENCE {

eventType-r16 EventType-r16,

loggingInterval-r16 LoggingInterval-r16,

...

}

EventType-r16 ::= CHOICE {

outOfCoverage NULL,

eventL1 SEQUENCE {

l1-Threshold MeasTriggerQuantity,

hysteresis Hysteresis,

timeToTrigger TimeToTrigger

},

...

}

-- TAG-LOGGEDMEASUREMENTCONFIGURATION-STOP

-- ASN1STOP

| ***LoggedMeasurementConfiguration* field descriptions** |
| --- |
| ***absoluteTimeInfo***  Indicates the absolute time in the current cell. |
| ***areaConfiguration***  Used to restrict the area in which the UE performs measurement logging to cells broadcasting either one of the included cell identities or one of the included tracking area codes/ frequencies. |
| ***eventType***  The value outOfCoverage indicates the UE to perform logging of measurements at regular time intervals as defined by the *loggingInterval* while the UE is in any cell selection state, and the value eventL1 indicates the UE to perform logging of measurements at regular time intervals as defined by the *loggingInterval* while the triggering condition as configured in the event is met for the camping cell in camped normally state. |
| ***plmn-IdentityList***  Indicates a set of PLMNs defining when the UE performs measurement logging as well as the associated status indication and information retrieval i.e. the UE performs these actions when the RPLMN is part of this set of PLMNs. |
| ***tce-Id***  Parameter Trace Collection Entity Id: See TS 32.422 [52]. |
| ***traceRecordingSessionRef***  Parameter Trace Recording Session Reference: See TS 32.422 [52]. |
| ***reportType***  Parameter configures the type of MDT configuration, specifically Periodic MDT conifguraiton or Event Triggerd MDT configuration. |