**3GPP TSG-RAN WG2 Meeting #113bis electronic R2-210xxxx**

**Online, April 12 – April 20, 2021**

**Title:** [Draft] LS on BCS for contiguous and non-contiguous intra-band (NG)EN-DC

**Response to:**

**Release:** Rel-15

**Work Item:** NR\_newRAT

**Source:** [Huawei, HiSilicon]

**To:** RAN4

**Cc:**

**Contact Person:**

**Name:** Yiru Kuang

**E-mail Address:** kuangyiru@huawei.com

**Attachments**: N/A

**1. Overall Description:**

RAN2 discussed bandwidth combination set (BCS) reporting for contiguous and non-contiguous intra-band (NG)EN-DC and concluded that:

If the UE supports an intra-band (NG)EN-DC band combination with both contiguous and non-contiguous configurations, and the supported BCS value(s)(e.g. BCS#0, BCS#1 and so on) for contiguous and non-contiguous is the same, the UE can signal “both” in *intraBandENDC-Support* with the associated BCS value(s);

If the supported BCS value(s) for contiguous and non-contiguous is different, the UE can signal two band combination entries for contiguous and for non-contiguous separately, with the associated BCS value(s) respectively;

If no BCS value(s) is signalled then the BCS#0 is assumed for a band combination.

**2. Actions:**

**To RAN4:**

**ACTION:** RAN2 respectfully asks RAN4 to take above RAN2 understanding into account.

**3. Date of Next TSG WG RAN2 Meetings:**

TSG-RAN2 Meeting#114-e 19 – 27 May 2021 Online

TSG-RAN2 Meeting#115-e 16 – 27 August 2021 Online