**3GPP TSG-RAN WG2 #113bis-e *R2-21xxxx***

**E-meeting, April 2021**

Agenda Item: 8.7.3

Source: Ericsson

Title: Summary of [602]

Document for: Discussion, Decision

# Introduction

This is to discuss the [706] as follows.

* [Post113bis-e][602][Relay] Definition of relay load criterion (Ericsson)

 Scope: Collect definitions of the relay load criterion and downselect candidates. Whether to use relay load as a criterion will not be discussed in this scope.

 Intended outcome: Report to next meeting

 Deadline: Long

For rapporteur to have enough time drafting summary report, we would like to have the following two phases:

* Phase 1: collect companies’ views by 2021-05-06 1000 UTC
* Phase 2: rapporteur will finalize summary report based on inputs of phase 1 by 2021-05-10 1000 UTC

# Discussion

The necessity of relay load has been initially discussed in [1], company views were summarized as the following.

* 14/25 companies (ZTE, QC, Ericsson, Sony, IDC, Sharp, MDK, Xiaomi, Vivo, FH, Apple, Kyocera, Philips, Convida) believe load indication would be beneficial, or are open to considering load as an additional AS criteria in case something simple can be specified.
* A number of other companies indicated their concern for being able to specify something simple with the limited time available.
* From the options for defining load provided in the question, it seems those with the most support are a, b, and f. These also seem to be the ones which can lead to the simplest solution. Rapporteur suggests RAN2 continue to discuss (e.g. based on contribution) whether load is considered as an additional AS criteria while downscoping the options to the most popular (a, b, and f) only.

*Proposal 1-1: RAN2 continue to discuss further whether to consider load as an additional AS criteria, based on specific details of using number of PC5 connections/remote UEs served by the relay and/or resource pool usage/capacity at the relay UE.*

The above proposal was not agreed due to lacking sufficient support. Therefore, the following discussions base on the outcome from [1] to further collect definition of load criterion from companies and perform possible down-selection.

## Selection criterion

From Rapporteur’s understanding, the definition of relay load criterion shall fulfil the following conditions

1. Simple and easy to compute
2. Reflecting performance that a remote UE could achieve if served by the relay UE candidate
3. Small spec change
4. low signaling overhead

Bullet a) is important to make sure that introduction of relay load criterion will not increase relay UE’s implementation complexity.

Fulfilling bullet b, remote UE will be able to determine if a relay UE candidate can meet remote UE’s performance requirements of the relay traffic. Relay UE’s capabilities and remote UEs’ capabilities can be considered accordingly. With Bullet c) and d), RAN2 puts least design efforts for defining relay load criterion.

**Q1-1: do companies agree that the definition of relay load criterion shall fulfil the following requirements?**

1. Simple and easy to compute
2. Reflecting performance that a remote UE could achieve if served by the relay UE candidate
3. Small spec change
4. Low signaling overhead
5. other

|  |  |  |
| --- | --- | --- |
| Company | Requirements of relay load criterion | Comments |
| Ericsson | a,b,c,d, |  |
|  |  |  |
|  |  |  |

## Definition of relay load criterion

Based on discussion outcome of clause 2.1, we list the most popular options which are indicated in [1] so that companies can do further evaluation and try to find a convergence among companies. In addition, companies are also welcomed to propose other options according to the requirements described in clause 2.1.

In this email discussion, Rapporteur refers the most popular options indicated in [1] (i.e., option a, b, and f) as Option 1, Option 2 and Option 3 in the below respectively.

**Option 1: Number of PC5 connections to Remote UEs currently being actively used for relaying**

**Option 2: Resource pool usage or capacity**

**Option 3: Number of remote UEs being served by the relay UE**

The above three options were not agreed in RAN2#113bis, mainly because that none of the options can reflect capabilities of relay UE and remote UEs which are being served by the relay UE. Therefore, the above options may not be able to indicate the real capacity or free bandwidth of relay UE candidate.

In addition, rapporteur would like to add an additional option, i.e.,

**Option 4** – **free bandwidth (or achievable bit rate) that relay UE can provide for relay traffic**.

In this option, a relay UE candidate can indicate how much bit rate or bandwidth a remote UE can achieve for its relay traffic if the remote UE connects to the relay UE candidate. This bit rate or bandwidth may be determined as the maximum bit rate/bandwidth of the relay UE candidate in Uu interface minus bit rate/bandwidth for relay traffic occupied by remote UEs which are being served by the relay UE in PC5 interfaces. This free bandwidth or achievable bit rate may be determined for UL relay traffic (i.e., from remote UE to gNB) and DL relay traffic (i.e., from gNB to remote UE) separately. In this option, relay UE candidate can estimate its maximum Uu bit rate/bandwidth based on implementation. It is feasible that relay UE candidate can perform estimation based on its radio channel quality or the historic UL grants or DL assignments. gNB may also provide assistance information (e.g. measure UL channel quality, and provide estimated UL bit rate to relay UE) accordingly.

In order to perform down-selection among the above options, Rapporteur would like to recommend companies to check whether each option can fulfill the requirements as described in clause 2.1.

**Q2-1: What requirements do companies believe that Option 1 is able to fulfil?**

1. Simple and easy to compute
2. Reflecting performance that a remote UE could achieve if served by the relay UE candidate
3. Small spec change
4. low signaling overhead
5. other

|  |  |  |
| --- | --- | --- |
| Company | Requirements of relay load criterion | Comments |
| Ericsson | a, c, d |  |
|  |  |  |
|  |  |  |

**Q2-2: What requirements do companies believe that Option 2 is able to fulfil?**

1. Simple and easy to compute
2. Reflecting performance that a remote UE could achieve if served by the relay UE candidate
3. Small spec change
4. low signaling overhead
5. other

|  |  |  |
| --- | --- | --- |
| Company | Requirements of relay load criterion | Comments |
| Ericsson | a, c, d |  |
|  |  |  |
|  |  |  |

**Q2-3: What requirements do companies believe that Option 3 is able to fulfil?**

1. Simple and easy to compute
2. Reflecting performance that a remote UE could achieve if served by the relay UE candidate
3. Small spec change
4. low signaling overhead
5. other

|  |  |  |
| --- | --- | --- |
| Company | Requirements of relay load criterion | Comments |
| Ericsson | a, c, d |  |
|  |  |  |
|  |  |  |

**Q2-4: What requirements do companies believe that Option 4 is able to fulfil?**

1. Simple and easy to compute
2. Reflecting performance that a remote UE could achieve if served by the relay UE candidate
3. Small spec change
4. low signaling overhead
5. other

|  |  |  |
| --- | --- | --- |
| Company | Requirements of relay load criterion | Comments |
| Ericsson | a, b, c, d |  |
|  |  |  |
|  |  |  |

Based on above questions, it is recommended to do down-selection of the options.

**Q2-5: According to the requirements as discussed in clause 2.1, which option do companies prefer for defining relay load criterion?**

**Option 1: Number of PC5 connections to Remote UEs currently being actively used for relaying**

**Option 2: Resource pool usage or capacity**

**Option 3: Number of remote UEs being served by the relay UE**

**Option 4: free bandwidth (or achievable bit rate) that relay UE can provide for relay traffic**

**Other options:**

|  |  |  |
| --- | --- | --- |
| Company | Option | Comments |
| Ericsson | Option 4 |  |
|  |  |  |
|  |  |  |

1. xxxxx.

# Conclusion

We have the following proposal:

[Proposal 1 xxxxx.](#_Toc70023351)

3.1 For chair notes (proposal in priority order)

# Reference

[1] [R2-2104414](file:///C%3A%5CUsers%5Cmtk16923%5CDocuments%5C3GPP%20Meetings%5C202104%20-%20RAN2_113bis-e%2C%20Online%5CExtracts%5CR2-2104414%20-%20%5B610%5D%5BRelay%5DAS_Criteria_reselection_summaryV2.docx) Summary of [AT113bis-e][610][Relay] AS criteria for relay (re)selection (InterDigital) InterDigital discussion

# Appendix