**3GPP TSG-RAN WG2 Meeting #115-e R2-210xxxx**

**E-Meeting, August 2021**

**Title: [Draft]** LS on UE ID in adaptation layer

**Response to:**

**Release:** Rel-17

**Work Item:** NR\_SL\_Relay-Core

**Source:** RAN2

**To:** SA3

**Cc:**

**Contact Person:**

#### Name: Boyuan Zhang

E-mail Address: <zhangboyuan@oppo.com>

**Send any reply LS to: 3GPP Liaisons Coordinator,** **mailto:3GPPLiaison@etsi.org**

**Attachments:** none

**1. Overall Description:**

Based on the following agreements from RAN2#113bis,

Proposal 3: For both DL and UL transmission of Uu radio bearers other than SRB0, **identity information of a remote UE** and its Uu radio bearer are included in the header of adaptation layer over Uu. FFS for SRB0. FFS if the presence of adaptation layer header can be configurable. (24/24)

Proposal 3b: The UE ID in the adaptation layer header is a local, temporary remote UE ID. FFS whether the **local, temporary remote UE ID** is assigned by the relay UE, or the serving gNB of the relay UE. (23/24)

RAN2 discussed how to configure the remote UE ID in the adaptation layer, and reached the following agreements during RAN2#115

Proposal 8 Serving gNB of relay UE assigns the local/temp remote UE ID.

**2. Actions:**

**To SA3**: RAN2 respectfully requests SA3 to take the above agreements into account.

**3. Dates of Next TSG-RAN WG2 Meetings:**

TSG RAN WG2 Meeting #116-e 1 November– 12 November 2021 eMeeting

TSG RAN WG2 Meeting #117 21 February – 25 February 2022 Athens, GR