**3GPP TSG-RAN WG2 Meeting #116bis Electronic *R2-220xxxx***

**Elbonia, 17 – 25 January 2022**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **37.340** | **CR** | **xxxx** | **rev** |  | **Current version:** | **16.7.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network | **X** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Introduction of the support for UDC in NR |
|  |  |
| ***Source to WG:*** | CATT, […] |
| ***Source to TSG:*** | R2 |
|  |  |
| ***Work item code:*** | NR\_UDC-Core |  | ***Date:*** | 2021-12 |
|  |  |  |  |  |
| ***Category:*** | **B** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | In 37.340 specification, it clarifies that in MR-DC, RoHC can be configured for all the bearer types. For UL data compression, the similar clarification should be also added in 37.340. |
|  |  |
| ***Summary of change:*** | Clarify that UDC can be configured for all the bearer types like RoHC. |
|  |  |
| ***Consequences if not approved:*** | UDC function would not be supported in NR Rel-17. |
|  |  |
| ***Clauses affected:*** | 6.3 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS 38.323 CR TS 38.331 CRTS 38.306 CRTS 38.300 CR |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** | Note this specification is not the latest version which should be updated later. |
|  |  |
| ***This CR's revision history:*** |  |

*First Change*

## 6.3 PDCP Sublayer

In EN-DC, CA duplication (see [3]) can be applied in the MN and in the SN, but MCG bearer CA duplication can be configured only in combination with E-UTRAN PDCP and MCG bearer CA duplication can be configured only if DC duplication is not configured for any split bearer.

In NGEN-DC, CA duplication can only be configured for SCG bearer. In NE-DC, CA duplication can only be configured for MCG bearer. In NR-DC, CA duplication can be configured for both MCG and SCG bearers, and can be configured together with DC duplication.

In MR-DC, RoHC, EHC and UDC (as described in TS 36.323 [15] and TS 38.323 [16]) can be configured for all the bearer types.

*End of Change*