3GPP TSG RAN WG2 Meeting #118-e R2-22xxxxx

e-Meeting, 9 - 20 May 2022

**Title: [DRAFT] LS on power-saving resource allocation with absent *sl-AllowedResourceSelectionConfig***

**Response to: -**

**Release: Release 17**

**Work Item: NR\_SL\_enh-Core**

**Source: vivo [To be RAN2]**

**To: RAN1**

**Cc: -**

**Contact person: Xiao XIAO**

**xiao.xiao@vivo.com**

**Send any reply LS to: 3GPP Liaisons Coordinator,** [**mailto:3GPPLiaison@etsi.org**](mailto:3GPPLiaison@etsi.org)

**Attachments:** **-**

# 1 Overall description

RAN2 discussed the intended UE behaviour in a resource pool for which *sl-AllowedResourceSelectionConfig* is absent. RAN2’s understanding is as follows:

* When the *sl-AllowedResourceSelectionConfig* is absent for a mode-2 transmission resource pool indicated by *sl-TxPoolSelectedNormal* (which can be included within *sl-BWP-PoolConfig-r16*/*sl-BWP-PoolConfigCommon-r16* and within *sl-BWP-PoolConfigPS-r17*/*sl-BWP-PoolConfigCommonPS-r17*, as specified in TS 38.331), the UE is only allowed to use full sensing based resource selection scheme for transmission in this resource pool.

# 2 Actions

**To RAN1**

**ACTION:** RAN2 would like to respectfully ask RAN1 to confirm the above RAN2’s understanding, and provide other feedback (if any concern).

# 3 Dates of next TSG RAN WG2 meetings

TSG RAN WG2 Meeting #119-e 15 August – 26 August 2022 e-Meeting

TSG RAN WG2 Meeting #119bis-e 10 October – 19 October 2022 e-Meeting