**3GPP TSG-RAN2 Meeting #118-eR2-2206712**

**Electronic, 9th – 20th May, 2022**

**Source: Email discussion Rapporteur (Huawei, HiSilicon)**

**Title: Summary for [Post118-e][502] UP open issues and CR to 38.321 (Huawei)**

**Agenda item:** **6.6.2**

**Document for:** **Discussion and Decision**

# General

This document contains the list of comments made during the review of the MAC CR for SDT

## Contacts

|  |  |  |
| --- | --- | --- |
| Name | Company | Email address |
| SeungJune Yi | LG Electronics | seungjune.yi@lge.com |
| Anil Agiwal | Samsung | anilag@samsung.com |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

### Comments

|  |  |  |  |
| --- | --- | --- | --- |
| Companies | Brief description of the issue | Suggested resolution/company comments | Proposed way forward by rapporteur |
| LG01 | 5.2  3> when the Contention Resolution is considered successful for Random Access procedure when the CG-SDT procedure is ongoing:  Double “when” is misleading | Change the second “when” to “while”.  3> when the Contention Resolution is considered successful for Random Access procedure while the CG-SDT procedure is ongoing: |  |
| LG02 | 5.2  1> when instruction from the upper layer has been received for indicating the expiry of the *cg-SDT-TimeAlignmentTimer*:  The text is not aligned with RRC text.  instruct the MAC entity to stop the *cg-SDT-TimeAlignmentTimer*, if it is running; | Align the text between RRC and MAC. Either using “expiring” or “stopping”.  If we choose to keep the RRC text, the MAC spec should keep the original text, i.e. “stopping”. |  |
| LG03 | 5.8.2  1> if, after initial transmission for CG-SDT with CCCH message has been performed according to clause 5.4.1, PDCCH addressed to the MAC entity's C-RNTI has not been received, and the SSB corresponding to the configured UL grant has the same SSB index as the SSB selected for initial transmission for CG-SDT with CCCH message (i.e., retransmission of initial transmission of CG-SDT);  3> if this is the initial transmission of CG-SDT with CCCH message after the CG-SDT procedure is initiated as in clause 5.27: (i.e., SSB selection for initial transmission for CG-SDT)  3> else if PDCCH addressed to C-RNTI has been received after the initial transmission of CG-SDT with CCCH message: (i.e., SSB for subsequent new transmission for CG-SDT)  Three highlighted texts are not aligned. | Remove “SSB selection for” from the second text and remove “SSB for” from the third text. |  |
| LG04 | 5.27.2  The MAC entity shall:  1> store the RSRP of the downlink pathloss reference derived based on the *measObject* configured for the Serving Cell as in TS 38.331 [5].  It is not clear when the MAC entity stores the RSRP. | Add the timing when the MAC entity stores the RSRP.  The MAC entity shall, upon reception of configuration for CG-SDT:  1> store the RSRP of the downlink pathloss reference derived based on the *measObject* configured for the Serving Cell as specified in TS 38.331 [5]. |  |
| Samsung001 | 5.27.1 General 2> if CG-SDT is configured on the selected UL carrier, and TA of the configured grant Type 1 resource is valid according to clause 5.27.2; and  2> if, for at least one RB configured for SDT having data available for transmission, *configuredGrantType1Allowed* is configured with value *true* for the corresponding logical channel(s); and  2> if at least one SSB configured for CG-SDT with SS-RSRP above *cg-SDT-RSRP-ThresholdSSB* is available:  3> indicate to the upper layers that the conditions for initiating SDT procedure are fulfilled;  3> perform CG-SDT procedure on the selected UL carrier according to clause 5.8.2.  We do not agree with this change. In our understanding, the intention of the agreement was to use LCH restriction (i.e. configuredGrantType1Allowed or allowedCG-List) for CG-SDT during the LCP procedure. It was not intended for CG-SDT vs RA-SDT selection. | Remove the change |  |
|  |  |  |  |