3GPP TSG-RAN WG2 Meeting #119-e R2-22xxxxx

Online, 17-26 August 2022

Source: Huawei, HiSilicon

Title: Summary of [Post][411][POS] Positioning 38.321 CR (Huawei)

# Issues for the CR

|  |  |  |  |
| --- | --- | --- | --- |
| **Company** | **Change** | **Issue in the CR** | **Propose TP** |
| *e.g., Huawei, HiSilicon* | *e.g., Change5* | *Xxx* | *xxx* |
| Ericsson | I wonder if the below needs to be updated to reflect that only when higher layers have configured schedulingRequestID, UE shall do the below:5.25 Positioning Measurement Gap Activation/Deactivation RequestIf the UE is configured with pre-configured measurement gap, the UE may request the network to activate or deactivate the Positioning measurement gap with UL MAC CE for Positioning Measurement Gap Activation/Deactivation Request in clause 6.1.3.40. |  | 5.25 Positioning Measurement Gap Activation/Deactivation RequestIf the UE is configured with pre-configured measurement gap and *schedulingRequestID-PosMG-Request* as specified inTS 38.331 [5] is configured, the UE may request the network to activate or deactivate the Positioning measurement gap with UL MAC CE for Positioning Measurement Gap Activation/Deactivation Request in clause 6.1.3.40. |

# Summary