**3GPP TSG-RAN WG2 Meeting #120R2-2213346**

**Meeting 14 – 18 November 2022**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  | **06** | **CR** | **0840** | **rev** | **1** | **Current version:** | **17.2.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network | **X** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Higher granularity for per-FR gap capability - Alt1.3b |
|  |  |
| ***Source to WG:*** | Qualcomm Incorporated |
| ***Source to TSG:*** | R2 |
|  |  |
| ***Work item code:*** | TEI17 |  | ***Date:*** | 11-14 |
|  |  |  |  |  |
| ***Category:*** | **C** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | In RAN2#119bis-e meeting, the chair’s recommended for the per-FR discussion (R2-2210450), delegates to provide CRs/TPs for the next meeting where CRs will provide solutions as proposed in Alt 1.3, Alt 1.3 per BC, Alt 2. Way Forward- Chair: Simplicity will be a decision criterion.- Chair: at first agreed to go offline, which was reverted - Chair: consider CRs/TPs for next meeting and finally decide then. * Exclude Alt 1.1 for now.
* On the table: Alt 1.3, Alt 1.3 per BC, Alt 2 (add info, based on current config as today, FFS excl/incl DC)

Subsequently, a discussion paper was submitted to this meeting (R2-2212526) highlighting the pros and cons of each proosed solution, and providing a new suggestion based on the Alt1.3 and Alt1.3a, solution “Alt1.3b” that does not have the caveats of the original ones, but inherited their benefits.  |
|  |  |
| ***Summary of change:*** | * Adding new capability IE “*independentGapConfig-maxCC-r17*” to inform the network about the max number of configured serving cells beyond which the network shall assume UE does not support *independ*entGapConfig capability.
* Adding the new inter-node messaging to coordinate the number of serving cells in MCG and SCG.

**Impact Analysis:**Impacted 5G architecture options: NR-SA, NR-DC, (NG)EN-DCImpacted functionality:Per FR gapInteroperability issue:* If the Network is implemented according to the CR and the UE is not, no interoperability issue is expected, as legacy behaviour is followed.
* If the UE is implemented according to the CR and the Network is not, no interoperability issue is expected, as network ignores the new capability.
 |
|  |  |
| ***Consequences if not approved:*** | The Per FR gap feature usage stays very limited. |
|  |  |
| ***Clauses affected:*** | 4.2.9 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** | **X** |  |  Other core specifications  | TS/TR 38.331 CR 3704 |
| ***affected:*** |  |  |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  |  |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

*Start of Changes*

4.2.9 *MeasAndMobParameters*

| **Definitions for parameters** | **Per** | **M** | **FDD-TDD DIFF** | **FR1-FR2 DIFF** |
| --- | --- | --- | --- | --- |
| ***cli-RSSI-Meas-r16***Indicates whether the UE can perform CLI RSSI measurements as specified in TS 38.215 [13] and supports periodical reporting and measurement event triggering as specified in TS 38.331 [9]. If the UE supports this feature, the UE needs to report *maxNumberCLI-RSSI-r16*. If this parameter is indicated for FR1 and FR2 differently, each indication corresponds to the frequency range of measurement resources to be measured. | UE | No | TDD only | Yes |
| ***cli-SRS-RSRP-Meas-r16***Indicates whether the UE can perform SRS RSRP measurements as specified in TS 38.215 [13] and supports periodical reporting and measurement event triggering based on SRS-RSRP as specified in TS 38.331 [9]. If the UE supports this feature, the UE needs to report *maxNumberCLI-SRS-RSRP-r16* and *maxNumberPerSlotCLI-SRS-RSRP-r16*. If this parameter is indicated for FR1 and FR2 differently, each indication corresponds to the frequency range of measurement resources to be measured. | UE | No | TDD only | Yes |
| ***concurrentMeasGap-r17***Indicates whether the UE supports the concurrent measurements gaps as specified in TS 38.133 [5]. The capability signalling comprises the following parameters:- *concurrentPerUE-OnlyMeasGap-r17* indicates whether the UE supports more than 1 per-UE measurement gap configurations (i.e. gap combination configuration id = 2 as specified in TS38.133 [5]), or*-* *concurrentPerUE-PerFRCombMeasGap-r17* indicates whether the UE supports all concurrent gap combination configurations as specified in TS 38.133 [5] including support of more than 1 per-UE measurement gap configurations. For UE capable of Rel-15 per-FR gap (*independentGapConfig*), this field indicates whether the UE supports more than 1 per-FR gap measurement gap configurations in an FR, or simultaneous 1 per UE measurement gap plus 1 per-FR measurement gap configurations in an FR, or more than 1 per-UE measurement gap configurations (i.e. gap combination configuration id = 2 as specified in TS38.133 [5]). | UE | No | No | No |
| ***concurrentMeasGapEUTRA-r17***Indicates whether the UE support the configurations of E-UTRAN measurement objectives associated with more than 1 concurrent measurement gaps as specified in TS 38.133 [5]. The UE indicating support of this feature shall also indicate support of *concurrentMeasGap-r17*. | UE | No | No | No |
| ***condHandoverFDD-TDD-r16***Indicates whether the UE supports conditional handover between FDD and TDD cells. The parameter can only be set if *condHandover-r16* is set for both FDD and TDD. The UE that indicates support of this feature shall also indicate support of *handoverFDD-TDD*. | UE | No | No | No |
| ***condHandoverFR1-FR2-r16***Indicates whether the UE supports conditional handover HO between FR1 and FR2. The parameter can only be set if *condHandover-r16* is set for both FR1 and FR2. The UE that indicates support of this feature shall also indicate support of *handoverFR1-FR2*. | UE | No | No | No |
| ***condHandoverWithSCG-NRDC-r17***Indicates whether the UE supports conditional handover with NR SCG configuration for NR-DC. The UE indicating support of this feature shall also indicate the support of *condHandover-r16* and support of at least one NR-DC band combination. | UE | No | No | No |
| ***csi-RS-RLM***Indicates whether the UE can perform radio link monitoring procedure based on measurement of CSI-RS as specified in TS 38.213 [11] and TS 38.133 [5]. This parameter needs FR1 and FR2 differentiation. If the UE supports this feature, the UE needs to report *maxNumberResource-CSI-RS-RLM*. This applies only to non-shared spectrum channel access. For shared spectrum channel access, *csi-RS-RLM-r16* applies. | UE | Yes | No | Yes |
| ***csi-RSRP-AndRSRQ-MeasWithSSB***Indicates whether the UE can perform CSI-RSRP and CSI-RSRQ measurement as specified in TS 38.215 [13], where CSI-RS resource is configured with an associated SS/PBCH. If this parameter is indicated for FR1 and FR2 differently, each indication corresponds to the frequency range of measured target cell. If the UE supports this feature, the UE needs to report *maxNumberCSI-RS-RRM-RS-SINR*. This applies only to non-shared spectrum channel access. For shared spectrum channel access, *csi-RS-RLM-r16* applies. | UE | No | No | Yes |
| ***csi-RSRP-AndRSRQ-MeasWithoutSSB***Indicates whether the UE can perform CSI-RSRP and CSI-RSRQ measurement as specified in TS 38.215 [13], where CSI-RS resource is configured for a cell that transmits SS/PBCH block and without an associated SS/PBCH block. If this parameter is indicated for FR1 and FR2 differently, each indication corresponds to the frequency range of measured target cell. If the UE supports this feature, the UE needs to report *maxNumberCSI-RS-RRM-RS-SINR*. This applies only to non-shared spectrum channel access. For shared spectrum channel access, *csi-RSRP-AndRSRQ-MeasWithoutSSB-r16* applies. | UE | No | No | Yes |
| ***csi-SINR-Meas***Indicates whether the UE can perform CSI-SINR measurements based on configured CSI-RS resources as specified in TS 38.215 [13]. If this parameter is indicated for FR1 and FR2 differently, each indication corresponding to the frequency range of measured target cell. If the UE supports this feature, the UE needs to report *maxNumberCSI-RS-RRM-RS-SINR*. This applies only to non-shared spectrum channel access. For shared spectrum channel access, *csi-SINR-Meas-r16* applies. | UE | No | No | Yes |
| ***eutra-AutonomousGaps-r16***Defines whether the UE supports, upon configuration of *useAutonomousGaps* by the network, acquisition of relevant information from a neighbouring E-UTRA cell by reading the SI of the neighbouring cell using autonomous gap and reporting the acquired information to the network as specified in TS 38.331 [9] when MR-DC is not configured.  | UE | No | No | No |
| ***eutra-AutonomousGaps-NEDC-r16***Defines whether the UE supports, upon configuration of *useAutonomousGaps* by the network, acquisition of relevant information from a neighbouring E-UTRA cell by reading the SI of the neighbouring cell using autonomous gap and reporting the acquired information to the network as specified in TS 38.331 [9] when NE-DC is configured. | UE | No | No | No |
| ***eutra-AutonomousGaps-NRDC-r16***Defines whether the UE supports, upon configuration of *useAutonomousGaps* by the network, acquisition of relevant information from a neighbouring E-UTRA cell by reading the SI of the neighbouring cell using autonomous gap and reporting the acquired information to the network as specified in TS 38.331 [9] when NR-DC is configured. | UE | No | No | No |
| ***eutra-CGI-Reporting***Defines whether the UE supports acquisition of relevant CGI-information from a neighbouring E-UTRA cell by reading the SI of the neighbouring cell and reporting the acquired information to the network as specified in TS 38.331 [9] when the (NG)EN-DC and NE-DC are not configured or, when consistent DRX is configured in NR-DC. The consistent DRX configuration implies that MN and SN have the same DRX cycle and on-duration configured by MN completely contains on-duration configured by SN. It is mandated if the UE supports EUTRA. It is optional for RedCap UEs. | UE | CY | No | No |
| ***eutra-CGI-Reporting-NEDC***Defines whether the UE supports acquisition of relevant information from a neighbouring E-UTRA cell by reading the SI of the neighbouring cell and reporting the acquired information to the network as specified in TS 38.331 [9] when theNE-DCis configured. | UE | No | No | No |
| ***eutra-CGI-Reporting-NRDC***Defines whether the UE supports acquisition of relevant information from a neighbouring E-UTRA cell by reading the SI of the neighbouring cell and reporting the acquired information to the network as specified in TS 38.331 [9] when theNR-DC is configured wherein MN and SN have different DRX cycles, or on-duration configured by MN does not contain on-duration configured by SN if the DRX cycles are the same. | UE | No | No | No |
| ***eutra-NeedForGapNCSG-reporting-r17***Indicates whether the UE supports reporting of the NCSG and measurement gap requirement information for E-UTRA target bands in the UE response to a network configuration RRC message as specified in TS 38.331 [9]. | UE | No | No | No |
| ***eventA-MeasAndReport***Indicates whether the UE supports NR measurements and events A triggered reporting as specified in TS 38.331 [9]. This field only applies to SN configured measurement when (NG)EN-DC is configured. For NR SA, MN and SN configured measurement when NR-DC is configured, and MN configured measurement when NE-DC is configured, this feature is mandatory supported. | UE | Yes | Yes | No |
| ***eventB-MeasAndReport***Indicates whether the UE supports EUTRA measurement and event B triggered reporting as specified in TS 38.331 [9]. It is mandated if the UE supports EUTRA. | UE | CY | No | No |
| ***gNB-ID-Length-Reporting-r17***Indicates whether the UE supports acquisition and reporting of gNB ID length from a neighbouring intra-frequency or inter-frequency NR cell by reading the SI of the neighbouring cell and reporting the acquired gNB ID length to the network as specified in TS 38.331 [9] when (NG)EN-DC and NE-DC are not configured or, when consistent DRX is configured in NR-DC. The consistent DRX configuration implies that MN and SN have the same DRX cycle and on-duration configured by MN completely contains on-duration configured by SN. It is mandated if UE supports NR CGI reporting (NG)EN-DC and NE-DC are not configured or, when consistent DRX is configured in NR-DC. | UE | CY | No | No |
| ***gNB-ID-Length-Reporting-ENDC-r17***Indicates whether the UE supports acquisition and reporting of gNB ID length from a neighbouring intra-frequency or inter-frequency NR cell by reading the SI of the neighbouring cell and reporting the acquired gNB ID length to the network as specified in TS 38.331 [9] when the (NG)EN-DC is configured. It is mandated if UE supports NR CGI reporting when (NG)EN-DC is configured. | UE | CY | No | No |
| ***gNB-ID-Length-Reporting-NEDC-r17***Indicates whether the UE supports acquisition and reporting of gNB ID length from a neighbouring intra-frequency or inter-frequency NR cell by reading the SI of the neighbouring cell and reporting the acquired gNB ID length to the network as specified in TS 38.331 [9] when the NE-DC is configured. It is mandated if UE supports NR CGI reporting when NE-DC is configured. | UE | CY | No | No |
| ***gNB-ID-Length-Reporting-NRDC-r17***Indicates whether the UE supports acquisition and reporting of gNB ID length from a neighbouring intra-frequency or inter-frequency NR cell by reading the SI of the neighbouring cell and reporting the acquired gNB ID length to the network as specified in TS 38.331 [9] when the NR-DC is configured wherein MN and SN have different DRX cycles, or on-duration configured by MN does not contain on-duration configured by SN if the DRX cycles are the same. It is mandated if UE supports NR CGI reporting when NR-DC is configured. | UE | CY | No | No |
| ***gNB-ID-Length-Reporting-NPN-r17***Indicates whether the UE supports acquisition of NPN-relevant gNB ID length from a neighbouring intra-frequency or inter-frequency NR NPN cell by reading the SI of the neighbouring cell and reporting the acquired gNB ID length to the network as specified in TS 38.331 [9]. It is mandated if UE supports NPN CGI reporting. | UE | CY | No | No |
| ***handoverLTE-5GC, handoverLTE-5GC-r17***Indicates whether the UE supports HO to EUTRA connected to 5GC. It is mandated if the UE supports EUTRA connected to 5GC. | UE | CY | Yes | Yes(Incl FR2-2 DIFF) |
| ***handoverFDD-TDD***Indicates whether the UE supports HO between FDD and TDD. It is mandated if the UE supports both FDD and TDD. This field only applies to NR SA/NR-DC/NE-DC (e.g. PCell handover). For PSCell change when (NG)EN-DC/NR-DC is configured, this feature is mandatory supported. UEs supporting this shall indicate support of *handoverInterF* for both FDD and TDD. | UE | Yes | No | No |
| ***handoverFR1-FR2***Indicates whether the UE supports HO between FR1 and FR2. Support is mandatory for the UE supporting both FR1 and FR2. This field only applies to NR SA/NR-DC/NE-DC (e.g. PCell handover). For PSCell change when (NG)EN-DC/NR-DC is configured, this feature is mandatory supported. UEs supporting this shall indicate support of *handoverInterF* for both FR1 and FR2. | UE | Yes | No | No |
| ***handoverFR1-FR2-2-r17***Indicates whether the UE supports HO between FR1 and FR2-2. This field only applies to NR SA/NR-DC/NE-DC (e.g. PCell handover) and PSCell change when (NG)EN-DC/NR-DC is configured. UEs supporting this shall indicate support of *handoverInterF* for both FR1 and FR2-2. | UE | No | No | No |
| ***handoverFR2-1-FR2-2-r17***Indicates whether the UE supports HO between FR2-1 and FR2-2. This field only applies to NR SA/NR-DC/NE-DC (e.g. PCell handover) and PSCell change when (NG)EN-DC/NR-DC is configured. UEs supporting this shall indicate support of *handoverInterF* for both FR2-1 and FR2-2. | UE | No | No | No |
| ***handoverInterF, handoverInterF-r17***Indicates whether the UE supports inter-frequency HO. It indicates the support for inter-frequency HO from the corresponding duplex mode and from frequency range indicated to be supported as described in Annex B. This field only applies to NR SA/NR-DC/NE-DC (e.g. PCell handover). For PSCell change when (NG)EN-DC/NR-DC is configured, this feature is mandatory supported. | UE | Yes | Yes | Yes(Incl FR2-2 DIFF) |
| ***handoverLTE-EPC, handoverLTE-EPC-r17***Indicates whether the UE supports HO to EUTRA connected to EPC. It is mandated if the UE supports EUTRA connected to EPC. | UE | CY | Yes | Yes(Incl FR2-2 DIFF) |
| ***idleInactiveNR-MeasReport-r16, idleInactiveNR-MeasReport-r17***Indicates whether the UE supports configuration of NR SSB measurements in RRC\_IDLE/RRC\_INACTIVE and reporting of the corresponding results upon network request as specified in TS 38.331 [9]. If this parameter is indicated for FR1 and FR2 differently, each indication corresponds to the frequency range of measured target cell. | UE | No | No | Yes(Incl FR2-2 DIFF) |
| ***idleInactiveNR-MeasBeamReport-r16***Indicates whether the UE supports beam level measurements in RRC\_IDLE/RRC\_INACTIVE and reporting of the corresponding beam measurement results upon network request as specified in TS 38.331 [9]. A UE supports this feature shall also support *idleInactiveNR-MeasReport-r16*. If this parameter is indicated for FR1 and FR2 differently, each indication corresponds to the frequency range of measured target cell. | UE | No | No | Yes |
| ***idleInactiveEUTRA-MeasReport-r16***Indicates whether the UE supports configuration of E-UTRA measurements in RRC\_IDLE/RRC\_INACTIVE and reporting of the corresponding results upon network request as specified in TS 38.331 [9]. | UE | No | No | No |
| ***idleInactive-ValidityArea-r16***Indicates whether the UE supports configuration of a validity area for NR measurements in RRC\_IDLE/RRC\_INACTIVE as specified in TS 38.331 [9]. | UE | No | No | No |
| ***independentGapConfig***This field indicates whether the UE supports two independent measurement gap configurations for FR1 and FR2 specified in clause 9.1.2 of TS 38.133 [5]. The field also indicates whether the UE supports the FR2 inter-RAT measurement without gaps when (NG)EN-DC is not configured. | UE | No | No | No |
| ***independentGapConfigPRS-r17***Indicates whether the UE supports two independent measurement gap configurations for FR1 and FR2 for PRS measurement, as specified in clause 9.1.2 of TS 38.133 [5]. | UE | No | No | No |
| ***independentGapConfig-maxCC-r17***indicates the maximum number of configured serving cells the UE supports with the *independentGapConfig* capability. if number of configured serving cells exceeds the maximum number indicated by this capability, network shall assume *independentGapConfig* capability is not supported by the UE for the current configuration.the capability signaling comprises the following parameters:* *N1* indicates the maximum number of configured serving cells when only FR1 serving cells are configured
* *N2* indicates the maximum number of configured serving cells when only FR2 serving cells are configured
* *N3* indicates the maximum number of configured serving cells when FR1 and FR2 serving cells are configured

The UE indicating support of this feature shall not indicate support of *independentGapConfig.* | UE | No | No | No |
| ***intraAndInterF-MeasAndReport***Indicates whether the UE supports NR intra-frequency and inter-frequency measurements and at least periodical reporting. This field only applies to SN configured measurement when (NG)EN-DC is configured. For NR SA, MN and SN configured measurement when NR-DC is configured, and MN configured measurement when NE-DC is configured, this feature is mandatory supported. | UE | Yes | Yes | No |
| ***interFrequencyMeas-NoGap-r16***Indicates whether the UE can perform inter-frequency SSB based measurements without measurement gaps if the SSB is completely contained in the active BWP of the UE as specified in TS 38.133 [5]. If this parameter is indicated for FR1 and FR2 differently, each indication corresponds to the frequency range of cells to be measured. | UE | No | No | Yes |
| ***periodicEUTRA-MeasAndReport***Indicates whether the UE supports periodic EUTRA measurement and reporting. It is mandated if the UE supports EUTRA. | UE | CY | No | No |
| ***maxNumberCLI-RSSI-r16***Defines the maximum number of CLI-RSSI measurement resources for CLI RSSI measurement. If the UE supports *cli-RSSI-Meas-r16*, the UE shall report this capability. | UE | CY | TDD only | No |
| ***maxNumberCLI-SRS-RSRP-r16***Defines the maximum number of SRS-RSRP measurement resources for SRS-RSRP measurement. If the UE supports *cli-SRS-RSRP-Meas-r16*, the UE shall report this capability.NOTE 1: A slot is based on minimum SCS among active BWPs across all CCs configured for SRS-RSRP measurement.NOTE 2: A SRS resource occasion that overlaps with the slot is counted as one measurement resource in the slot. | UE | CY | TDD only | No |
| ***increasedNumberofCSIRSPerMO-r16***Indicates support of up to 192 CSI-RS resource for L3 mobility configuration per measurement object configured with *associatedSSB*. | UE | No | No | Yes |
| ***maxNumberCSI-RS-RRM-RS-SINR***Defines the maximum number of CSI-RS resources for RRM and RS-SINR measurement across all measurement frequencies per slot. If UE supports any of *csi-RSRP-AndRSRQ-MeasWithSSB*, *csi-RSRP-AndRSRQ-MeasWithoutSSB*, and *csi-SINR-Meas*, UE shall report this capability.NOTE: A slot is based on minimum SCS among all measurement frequencies configured for RRM and RS-SINR measurement. | UE | CY | No | No |
| ***maxNumberPerSlotCLI-SRS-RSRP-r16***Defines the maximum number of SRS-RSRP measurement resources per slot for SRS-RSRP measurement. If the UE supports *cli-SRS-RSRP-Meas-r16*, the UE shall report this capability. | UE | CY | TDD only | No |
| ***maxNumberResource-CSI-RS-RLM***Defines the maximum number of CSI-RS resources within a slot per spCell for CSI-RS based RLM. If UE supports any of *csi-RS-RLM* and *ssb-AndCSI-RS-RLM*, UE shall report this capability. | UE | CY | No | Yes |
| ***ncsg-MeasGapNR-Patterns-r17***Indicates whether the UE supports NR-only NCSG patterns. The left most bit in the bitmap corresponds to NCSG pattern #0 and the right most bit in the bitmap corresponds to NCSG pattern #23. A bit in the bitmap is set to 1 if the corresponding pattern is supported by the UE. NCSG patterns #0 to #23 are as specified in TS38.133 [5].NCSG patterns #2 and #3 are mandatory (i.e. the corresponding bits in the bitmap is set to 1) if the UE includes this field. NCSG patterns #17 and #18 are mandatory (i.e. the corresponding bits in the bitmap is set to 1) if UE includes this field and supports a FR2 band. UEs supporting this shall indicate support of *nr-NeedForGapNCSG-reporting-r17*. | UE | No | No | No |
| ***ncsg-MeasGapPatterns-r17***Indicates whether the UE supports NCSG patterns. The left most bit in the bitmap corresponds to NCSG pattern #0 and the right most bit in the bitmap corresponds to NCSG pattern #23. A bit in the bitmap is set to 1 if the corresponding pattern is supported by the UE. NCSG patterns #0 to #23 are as specified in TS38.133 [5].NCSG patterns #0 and #1 are mandatory (i.e. the corresponding bits in the bitmap is set to 1) if the UE includes this field. NCSG patterns #13 and #14 are mandatory (i.e. the corresponding bits in the bitmap is set to 1) if UE supports *ncsg-MeasGapPerFR-r17* or if the UE is NCSG capable and supports FR2 band in standalone mode. UEs supporting this shall indicate support of *nr-NeedForGapNCSG-reporting-r17* and *eutra-NeedForGapNCSG-reporting-r17*. | UE | No | No | No |
| ***ncsg-MeasGapPerFR-r17***Indicates whether the UE supports per-FR NCSG. UEs supporting this shall indicate support of *nr-NeedForGapNCSG-reporting-r17*. | UE | No | No | No |
| ***ncsg-SymbolLevelScheduleRestrictionInter-r17***Indicates whether the UE supports performing measurement with NCSG based on flag *deriveSSB-IndexFromCell-inter* and meeting the following requirements that the scheduling restriction in FR2 serving cell during NCSG ML is on SSB symbol level. UEs supporting this shall indicate support of *nr-NeedForGapNCSG-reporting-r17*. | UE | No | No | FR2 only |
| ***nr-AutonomousGaps-r16***Defines whether the UE supports, upon configuration of *useAutonomousGaps* by the network, acquisition of relevant information from a neighbouring NR cell by reading the SI of the neighbouring cell using autonomous gap and reporting the acquired information to the network as specified in TS 38.331 [9] when MR-DC is not configured. If this parameter is indicated for FR1 and FR2 differently, each indication corresponds to the frequency range of measured target cell. | UE | No | No | Yes |
| ***nr-AutonomousGaps-ENDC-r16***Defines whether the UE supports, upon configuration of *useAutonomousGaps* by the network, acquisition of relevant information from a neighbouring NR cell by reading the SI of the neighbouring cell using autonomous gap and reporting the acquired information to the network as specified in TS 38.331 [9] when (NG)EN-DC is configured. If this parameter is indicated for FR1 and FR2 differently, each indication corresponds to the frequency range of measured target cell. | UE | No | No | Yes |
| ***nr-AutonomousGaps-NEDC-r16***Defines whether the UE supports, upon configuration of *useAutonomousGaps* by the network, acquisition of relevant information from a neighbouring NR cell by reading the SI of the neighbouring cell using autonomous gap and reporting the acquired information to the network as specified in TS 38.331 [9] when NE-DC is configured. If this parameter is indicated for FR1 and FR2 differently, each indication corresponds to the frequency range of measured target cell. | UE | No | No | Yes |
| ***nr-AutonomousGaps-NRDC-r16***Defines whether the UE supports, upon configuration of *useAutonomousGaps* by the network, acquisition of relevant information from a neighbouring NR cell by reading the SI of the neighbouring cell using autonomous gap and reporting the acquired information to the network as specified in TS 38.331 [9] when NR-DC is configured. If this parameter is indicated for FR1 and FR2 differently, each indication corresponds to the frequency range of measured target cell. | UE | No | No | Yes |
| ***nr-CGI-Reporting***Defines whether the UE supports acquisition of relevant CGI-information from a neighbouring intra-frequency or inter-frequency NR cell by reading the SI of the neighbouring cell and reporting the acquired information to the network as specified in TS 38.331 [9] when (NG)EN-DC and NE-DC are not configured or, when consistent DRX is configured in NR-DC. The consistent DRX configuration implies that MN and SN have the same DRX cycle and on-duration configured by MN completely contains on-duration configured by SN. It is optional for RedCap UEs. | UE | Yes | No | No |
| ***nr-CGI-Reporting-ENDC***Defines whether the UE supports acquisition of relevant CGI-information from a neighbouring intra-frequency or inter-frequency NR cell by reading the SI of the neighbouring cell and reporting the acquired information to the network as specified in TS 38.331 [9] when the (NG)EN-DC is configured. | UE | Yes | No | No |
| ***reportAddNeighMeasForPeriodic-r16***Defines whether the UE supports periodic reporting of best neighbour cells per serving frequency, as defined in TS 38.331 [9]. It is optional for RedCap UEs. | UE | Yes | No | No |
| ***nr-CGI-Reporting-NEDC***Defines whether the UE supports acquisition of relevant information from a neighbouring intra-frequency or inter-frequency NR cell by reading the SI of the neighbouring cell and reporting the acquired information to the network as specified in TS 38.331 [9] when the NE-DC is configured. | UE | Yes | No | No |
| ***nr-CGI-Reporting-NPN-r16***Defines whether the UE supports acquisition of NPN-relevant CGI-information from a neighbouring intra-frequency or inter-frequency NR NPN cell by reading the SI of the neighbouring cell and reporting the acquired information to the network as specified in TS 38.331 [9]. If UE supports NPN, UE shall report this capability. It is optional for RedCap UEs. | UE | CY | No | No |
| ***nr-CGI-Reporting-NRDC***Defines whether the UE supports acquisition of relevant information from a neighbouring intra-frequency or inter-frequency NR cell by reading the SI of the neighbouring cell and reporting the acquired information to the network as specified in TS 38.331 [9] when the NR-DC is configured wherein MN and SN have different DRX cycles, or on-duration configured by MN does not contain on-duration configured by SN if the DRX cycles are the same. | UE | Yes | No | No |
| ***nr-NeedForGapNCSG-reporting-r17***Indicates whether the UE supports reporting of the NCSG and measurement gap requirement information for SSB based measurement in the UE response to a network configuration RRC message as specified in TS 38.331 [9]. | UE | No | No | No |
| ***nr-NeedForGap-Reporting-r16***Indicates whether the UE supports reporting the measurement gap requirement information for NR target in the UE response to a network configuration RRC message. | UE | No | No | No |
| ***parallelMeasurementGap-r17***Indicates whether the UE supports 2 parallel measurement gaps for NTN RRM measurements. If a UE does not include this field but includes *nonTerrestrialNetwork-r17*, the UE supports 1 measurement gap for NTN RRM measurements. If this parameter is indicated, a UE shall also support that two parallel measurement gaps with the same gap type can be associated to one frequency layer. A UE supporting this feature shall also indicate the support of *nonTerrestrialNetwork-r17*. | UE | No | FDD only | FR1 only |
| ***parallelSMTC-r17***Indicates whether the UE supports NTN RRM measurements on target cells belonging to 4 SMTC-s on a single frequency carrier. If a UE does not include this field but includes *nonTerrestrialNetwork-r17*, the UE supports NTN RRM measurements on target cells belonging to 2 SMTC-s on a single frequency carrier. | UE | No | FDD only | FR1 only |
| ***pcellT312-r16***Indicates whether the UE supports T312 based fast failure recovery for PCell. | UE | No | No | No |
| ***preconfiguredUE-AutonomousMeasGap-r17***Indicates whether the UE supports the preconfigured measurement gap with UE-autonomous mechanism for activation and deactivation as specified in TS 38.133 [5]. | UE | No | No | No |
| ***preconfiguredNW-ControlledMeasGap-r17***Indicates whether the UE supports the preconfigured measurement gap with network-controlled mechanism for activation and deactivation as specified in TS 38.133 [5]. | UE | No | No | No |
| ***serviceLinkPropDelayDiffReporting-r17***Indicates whether the UE supports the reporting of service link propagation delay difference between serving cell and neighbour cell(s). A UE supporting this feature shall also indicate the support of *nonTerrestrialNetwork-r17*. | UE | No | No | No |
| ***simultaneousRxDataSSB-DiffNumerology***Indicates whether the UE supports concurrent intra-frequency measurement on serving cell or neighbouring cell and PDCCH or PDSCH reception from the serving cell with a different numerology as defined in clause 8 and 9 of TS 38.133 [5]. | UE | No | No | Yes |
| ***simultaneousRxDataSSB-DiffNumerology-Inter-r16***Indicates whether the UE supports concurrent SSB based inter-frequency measurement without measurement gap on neighbouring cell and PDCCH or PDSCH reception from the serving cell with a different numerology as defined in clause 8 and 9 of TS 38.133 [5]. UE indicates support of this indicates support of *interFrequencyMeas-NoGap-r16*. If this parameter is indicated for FR1 and FR2 differently, each indication corresponds to the frequency range where the SSB and PDCCH/PDSCH are received. | UE | No | No | Yes |
| ***sftd-MeasPSCell***Indicates whether the UE supports SFTD measurements between the PCell and a configured PSCell. If this capability is included in UE-MRDC-Capability, it indicates that the UE supports SFTD measurement between PCell and PSCell in (NG)EN-DC. If this capability is included in UE-NR-Capability, it indicates that the UE supports SFTD measurement between PCell and PSCell in NR-DC. | UE | No | Yes | No |
| ***sftd-MeasPSCell-NEDC***Indicates whether the UE supports SFTD measurement between the NR PCell and a configured E-UTRA PSCell in NE-DC. | UE | No | Yes | No |
| ***sftd-MeasNR-Cell***Indicates whether the SFTD measurement with and without measurement gaps between the EUTRA PCell and the NR cells is supported by the UE which is capable of EN-DC/NGEN-DC when EN-DC/NGEN-DC is not configured. The SFTD measurement without gaps can be used when the UE supports at least one EN-DC band combination consisting of the set of the current E-UTRA serving frequencies and the NR frequency where SFTD measurement is configured. In UE-NR-Capability, this field is not used, and UE does not include the field. | UE | No | Yes | No |
| ***sftd-MeasNR-Neigh***Indicates whether the inter-frequency SFTD measurement with and without measurement gaps between the NR PCell and inter-frequency NR neighbour cells is supported by the UE when MR-DC is not configured. The SFTD measurement without gaps can be used when the UE supports at least one DC or CA band combination consisting of the set of the current NR serving frequencies and the NR frequency where SFTD measurement is configured.  | UE | No | Yes | No |
| ***sftd-MeasNR-Neigh-DRX***Indicates whether the inter-frequency SFTD measurement using DRX off period between the NR PCell and the inter-frequency NR neighbour cells is supported by the UE when MR-DC is not configured. | UE | No | Yes | No |
| ***ssb-RLM***Indicates whether the UE can perform radio link monitoring procedure based on measurement of SS/PBCH block as specified in TS 38.213 [11] and TS 38.133 [5]. This field shall be set to *supported*. This applies only to non-shared spectrum channel access. For shared spectrum channel access, *ssb-RLM-DynamicChAccess-r16* or *ssb-RLM-Semi-StaticChAccess-r16* applies. | UE | Yes | No | No |
| ***ssb-AndCSI-RS-RLM***Indicates whether the UE can perform radio link monitoring procedure based on measurement of SS/PBCH block and CSI-RS as specified in TS 38.213 [11] and TS 38.133 [5]. If the UE supports this feature, the UE needs to report *maxNumberResource-CSI-RS-RLM*. This applies only to non-shared spectrum channel access. For shared spectrum channel access, *ssb-AndCSI-RS-RLM-r16* applies. | UE | No | No | No |
| ***ss-SINR-Meas***Indicates whether the UE can perform SS-SINR measurement as specified in TS 38.215 [13]. If this parameter is indicated for FR1 and FR2 differently, each indication corresponds to the frequency range of measured target cell. This applies only to non-shared spectrum channel access. For shared spectrum channel access, *ss-SINR-Meas-r16* applies. | UE | No | No | Yes |
| ***supportedGapPattern***Indicates measurement gap pattern(s) optionally supported by the UE for NR SA, for NR-DC, for NE-DC and for independent measurement gap configuration on FR2 in (NG)EN-DC. The leading / leftmost bit (bit 0) corresponds to the gap pattern 2, the next bit corresponds to the gap pattern 3, as specified in TS 38.133 [5] and so on. The UE shall set the bits corresponding to the measurement gap pattern 13, 14, 17, 18 and 19 to 1 if the UE is an NR standalone capable UE that supports a band in FR2 or if the UE is an (NG)EN-DC capable UE that supports *independentGapConfig* and supports a band in FR2. | UE | CY | No | No |
| ***supportedGapPattern-r16***Indicates measurement gap pattern(s) optionally supported by the UE for NR SA, for NR-DC for PRS measurement and NR/E-UTRA RRM measurement. The leading / leftmost bit (bit 0) corresponds to the gap pattern 24, the next bit corresponds to the gap pattern 25, as specified in TS 38.133 [5]. The applicability of the gap patterns 24 and 25 is defined in clause 9.1.2 of TS 38.133 [5]. A UE that indicates support of this capability shall indicate support of *NR-DL-PRS-ProcessingCapability-r16* defined in TS 37.355 [22]. | UE | No | No | No |
| ***supportedGapPattern-NRonly-r16***Indicates measurement gap pattern(s) optionally supported by the UE for NR SA and NR-DC when the frequencies to be measured within this measurement gap are all NR frequencies. The leading / leftmost bit (bit 0) corresponds to the gap pattern 2, the next bit corresponds to the gap pattern 3 and so on. The UE shall set the bits corresponding to the measurement gap pattern 2, 3 and 11 to 1. | UE | FD | No | No |
| ***supportedGapPattern-NRonly-NEDC-r16***Indicates whether the UE supports gap patterns 2, 3 and 11 in NE-DC when the frequencies to be measured within this measurement gap are all NR frequencies. | UE | No | No | No |

*End of Changes*