**3GPP TSG RAN2 #121 R2-23xxxxx**

**Athens, Greece, 27th Feb – 3rd Mar, 2023**

**Agenda Item:**  **XX.YY**

**Source: Huawei (email rapporteur)**

**Title:** **Report of [Post120][313][UAV] Interference Control for UAVs (Huawei)**

**Document for: Discussion and Decision**

# 1 Introduction

This is the report of the email discussion[Post120][313]:

* [Post120][313][UAV] Interference Control for UAVs (Huawei)

Scope: Discuss the following aspects:

- Number of triggering cells: Scenarios (e.g. inter-RAT), possible modification compared to LTE baseline (need, motivation, option, benefit/drawback). Applicability to FR1/FR2 and need for ignoring mechanism (e.g. one cell is particularly strong). Discuss need for alternative mechanisms (number of changed cell, prohibit timer etc.

- CellsTriggeredList: possible modification compared to the LTE baseline (Motivation, options, claimed benefits and possible drawbacks). E.g. numberOfTriggeringCellsForLeaving.

Output: set of agreeable proposals

Deadline: Long - Kick off: Jan 9th, Deadline for company inputs Jan, 20th. Inactive Period January 23 to 27. Comments on rapporteur summary Jan. 30th to February 3rd

All the relevant documents from previous RAN2 meetings have been taken into account, nevertheless for the sake of progress we should focus a bit, and not all the proposals submitted in the past are in the scope of this email discussion. So please do not “expand” the scope of this email discussion. Please remember to justify your answer with clear motivations, expected gains/drawback, etc. Where applicable, rather than copying a lot of explanatory text, you can reference your (or somebody else) paper if needed.

Companies are invited to put their comment in the file and change the file name in the folder according to the convention below:

File\_v00\_Rapp

File\_v01\_company1

File\_v02\_company2

…

File location:

hyperlink

PS: As a reminder, I copy here the latest agreement relevant to this email discussion. The purpose of *numberOfTriggeringCells* mechanism is to limit the interference caused by too many (measurement) reports.

Agreement in RAN2#119bis:

1. As in LTE, as a baseline, events A3, A4 and A5 can be configured with the configured number of cells (numberofTriggeringCells)

Companies providing input to this email discussion are invited to leave contact information below.

|  |  |  |
| --- | --- | --- |
| **Company** | **Name** | **Email Address** |
| Rapporteur | Simone Provvedi | Simone.provvedi@huawei.com |
| Huawei, HiSilicon | Jie Li | Lijie363@huawei.com |
| Ericsson | Helka-liina Määttänen | Helka-liina.maattanen@ericsson.com |
| Qualcomm | Umesh Phuyal | uphuyal@qti.qualcomm.com |
| LGE | Soo Kim | soo.kim@lge.com |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

# 2 Discussion

## 2.1 Applicability to the inter-RAT scenario

RAN2 should decide if the Number of triggering cells mechanism should be extended to apply to the inter-RAT scenario, i.e. event B1 and B2 triggering. How likely is that the UE will move at the border between LTE and NR? And what should we do in that case? If the Number of triggering cells mechanism is used, would this affect negatively the mobility, in particular the inter-RAT HO?

**Q1: Do you think that the Number of triggering cells mechanism should be extended to apply to the inter-RAT scenario, i.e. event B1 and B2 triggering?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Short answer** | **Comments** |
| Huawei, HiSilicon | No | The inter-RAT scenario should not occur too frequently compared to the intra-RAT, but more importantly if we extend the *numberofTriggeringCells* mechanism to the inter-RAT scenario we see a risk for HO failure at the cross between the two different RAT, given by the UE withholding its measurement report in some cases.  |
| Ericsson | Yesyes | But we would like to clarify that the RSRP report triggering based on number of cells is not for mobility but for interference/flying mode detection.When triggering is based on N cells, all Ncells need to trigger before the measurement report is sent. Hence, the report is way delayed for mobility purposes! Actually, for mobility, short TTT is beneficial when UE is flying as the cell coverage gets scattered on higher altitudes.That, said, in our view taking into account LTE and NR cells in detecting interference and/or flying mode is important. |
| Qualcomm | No strong view |  |
| LGE | No strong view |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

## 2.2 Applicability to FR1/FR2

RAN2 should decide if the applicability of Number of triggering cells mechanism should be restricted to FR1 only.

**Q2: Do you think that the applicability of Number of triggering cells mechanism should be restricted to FR1 only? Why yes/why not?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Short answer** | **Comments** |
| Huawei, HiSilicon | No | We do not see a reason why the *numberofTriggeringCells* mechanism should be restricted in FR1. Ultimately this is could be left to network configuration. |
| Ericsson | No | It would be important UE considers all cell in vicinity to trigger based on N cells. |
| Qualcomm | No | If we end up defining the mechanisms, we do not see a need to restrict it to FR1 only. It is up to the network to decide and configure accordingly. |
| LGE | No | We think there is no reason to restrict the mechanism by frequency range. The network can configure an appropriate *numberofTriggeringCells* according to the frequency range.  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

## 2.3 Need for ignoring or bypassing the Number of triggering cells mechanism

RAN2 should decide if there is a need for ignoring or bypassing the Number of triggering cells mechanism, once configured (e.g. for the case of strong DL interference from some neighbour cells, or the UE altitude is too high/not too high, or…).

**Q3: Do you think that the there is a need for the UE to ignore or bypass the Number of triggering cells mechanism, once configured, in some cases? If yes, in which cases and why?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Short answer** | **Comments** |
| Huawei, HiSilicon | Yes | As we all know, introducing the number of triggering cells mechanism can result in late handover. Thus, in some scenarios we need to skip the number of triggering cells mechanism to ensure the network obtains the measurement report in time. For example, if the number of cells in the cellsTriggeredList is smaller than the *numberofTriggeringCells* when the UAV detects the DL interference of a certain cell as being very strong (i.e. signal level above a threshold), the UAV should send the measurement report to the network immediately, to ensure the network takes the appropriate actions on time. |
| Ericsson | No | Regular events need to be configured for the UE in addition to N of triggering cells for mobility support. This was the understanding already in LTE. (For the regular event, one can consider further enhancements mobility support) |
| Qualcomm | No | UE follows what network configures (including any new mechanism that may be introduced in R18). If there is desire and consensus for the UE to behave in a certain way, e.g. for the case of strong DL interference from some neighbour cells, then there should be corresponding procedure and configuration for that case, and UE again follows the configuration as specified (this is not same as UE ignoring or bypassing autonomously the configuration of number of triggering cells mechanism). |
| LGE | Yes  | If the DL interference by a few neighbor cell is too strong, UE may face problems before sending measurement reports such as decoding failure due to interference. Therefore, in the case of strong DL interference from neighbor cells, UE should be able to report strong DL interference even when the number of neighbour cells does not satisfy the *numberOfTriggeringCells*. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

## 2.4 Need for introducing an alternative mechanism to the Number of triggering cells one.

RAN2 should discuss if there is a need for an alternative mechanism to the Number of triggering cells one (need, motivation, options, benefit/drawback). In particular it has been mentioned as alternative a mechanism based on

“Number of changed cells”.

**Q4: Do you see the need for an alternative mechanism to the Number of triggering cells one? In particular what is your opinion on a mechanism based on “Number of changed cells”?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Short answer** | **Comments** |
| Huawei, HiSilicon | No | For the entry condition, we think the number of changed cells is almost equivalent to the *numberofTriggeringCells*. RAN2 has been agreed to introduce the *numberofTriggeringCells* for LTE in the past and now that’s the baseline for NR*.* As a result, there is no reason to introduce the number of changed cells.For the leaving condition, using number of changed cells may cause the wrong HO. Assume the number of changed cells is two, and cells A, B, and C are in the cellsTriggeredList and has been reported to the network. When cell A leaves the list, the UE will not send measurement report, and if the network hands over the drone to cell A at this moment, this will result in handover failure. |
| Ericsson | No | Alternative mechanism for what use? For interference detection we have this and it seems enough. For flying mode detection we have this and H events. For mobility, we have the other email discussion to consider what is needed for that. |
| Qualcomm | No | RAN2 agreed to number of triggering cells mechanism after studying and analysing various simulation results for LTE in Rel-15 and recently agreed to re-use it for NR. We do not see need and motivation to introduce alternative mechanism based on number of changed cells. |
| LGE | Yes | In LTE, the UE cannot send another measurement for that measurement ID if the number of cells satisfies the number of triggering cells. We can discuss how to continuously and efficiently notify interference after the first measurement report. From this perspective, an alternative mechanism can be useful. Report restriction always has a trade-off relationship with handover failure. When the “number of change list” is applied to only one entry or leaving condition, the network can set an appropriate value according to the frequency characteristics or the situation the UE is in. Even, without limiting entry/leaving condition, if changes are counted by considering all added or removed cells from a list in the previous report, the environment the UE is in may be well reflected. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

## 2.5 Need for introducing a prohibit timer.

RAN2 should discuss if there is a need for a prohibit timer mechanism. What would be the motivation, the expected gains and drawbacks. Should this be introduced in coexistence or as an alternative to the baseline CellsTriggered mechanism?

**Q5: Do you see the need for introducing a prohibit timer mechanism?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Short answer** | **Comments** |
| Huawei, HiSilicon | Yes | We believe that the cellsTriggered mechanism and the prohibit timer can coexist. Using the prohibit timer mechanism in combination with the cell Triggered mechanism can reduce the measurement reports even further.For example, if the prohibit timer expires but the number of cells is less than the *numberOfTriggeringCells*, the UAV will continue to refrain from sending reports*.* Otherwise, it will send the reports. Also the other way around works, i.e. the UE can follow the most restrictive conditions of the two.  |
| Ericsson | Yes | This is proposed for regular mobility events originally!This method can control the amount of measurement reporting, also at the same time it enables timely reporting when the event is triggered first time.Preventing certain measurement results may result in a worry on decreasing mobility performance, but we have results in R2-1807257 to prove that it is not a problem. |
| Qualcomm | No | If there are too many measurement reports triggered due to certain network configuration, the correct approach is to adjust the configuration by the network instead of ‘*prohibit*’ing the reports by yet another new configuration (which are legitimately triggered by the network configuration). Prohibiting the reports also does not solve the issue of UE having to perform the measurements in the first place.  |
| LGE | No | We think the prohibit timer is not suitable for reporting interference. Even the configured timer may not be suitable depending on the speed of the UE. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

## 2.6 reportOnLeave.

RAN2 should discuss the reportOnLeave mechanism.

Is the LTE baseline suitable/sufficient? If not, which of the following enhancements will make sense to introduce and why? Indicate possible gains and drawbacks in your view. In particular your opinion is welcome on the following:

1. Introduce a numberOfTriggeringCellsForLeaving
2. The UE should not report a cell leaving if that cell was not reported joining previously.
3. Measurement report when the number of cells in *cellsTriggeredList* becomes smaller than a threshold

**Q6: Do you see the need to enhance the reportOnLeave mechanism? Please comment on the possible enhancements listed above.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Short answer** | **Comments** |
| Huawei, HiSilicon | b | Solutions a) and c) may cause the wrong HO, like the number of changed cells. See for example our comments in the papers that we submitted in Q4 for more details.For solution b), we think this mechanism should work (i.e. be introduced) only when the number of cells in the CellsTriggereddList is greater than *numberOfTriggeringCells.* When the number of cells is smaller than *numberOfTriggeringCells* should follow the current mechanism, i.e., the UAV sends a report to the network when a cell leaves. In this way we do not see any technical drawbacks and some useless measurement reports can be avoided. |
| Ericsson | See comment | If numberOfTriggeringCellsForLeaving means a measurement report is triggered when the number of cells in the list goes below this value it seems ok to consider. |
| Qualcomm | b + c | Motivation for a) is not convincing enough to justify the additional complexity/work to introduce the new procedures. |
| LGE | a | For option b, if the leaving condition is applied only to the cells included in the previous measurement reports, it is difficult to notify the interference continuously. The leaving condition can be a complement to sending measurement reports when measurement reports cannot be sent due to the number of triggering cells condition. Therefore, to inform the interference continuously, the UE must be able to report the interference regardless of whether the cell has been previously reported. For option c, we think, even if there are more cells than a certain threshold, a report is required if large interference is measured or there is a large change in the list.Therefore, we think ‘option a’ seems to be reasonable to report the interference continuously while preventing an excessive report. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

## 2.7 Use of “beams” vs “cells” for interference control.

RAN2 should discuss the possible use of “beams” vs “cells” for interference control. Will this increase the number of reports, and therefore the interference, or rather the opposite? How would that work? What are the possible gains and drawbacks?

**Q7: Do you see the need to use of “beams” instead of “cells” for interference control?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Short answer** | **Comments** |
| Huawei, HiSilicon | No | In NR, the measurement report is still based on the measurement result at the cell level, even for the beamforming cell. Thus, using beams for interference control cannot improve the performance of interference control. We see that this could cause additional work in RAN2 for no real benefit. |
| Ericsson | No | It’s a bit unclear what is meant by “interference control”. In general, in NR the measurements are done at beam level and the measurements can be used to calculate a cell-level quantities. In our view, using cell-level RSRP is appropriate for the event of numberOfTriggeringCells.  |
| Qualcomm | See comments | The question is a bit confusing. The beam level measurements can be used to calculate cell-level quantities, and such cell-level value is appropriate for the evaluation of event trigger conditions for numberOfTriggeringCells. However, if beam level reporting is considered, then separate trigger condition e.g. numberOfTriggeringBeams would be needed. Note that we showed previously that naturally there will be more measurements when there is more than one beam per cell (compared to one beam per cell). So, if report trigger mechanisms depend on number of ‘beams’, for example, instead of number of ‘cells’, there will be more reports triggered. We observed that measuring only a subset of beams based on height can save on number of measurements without significant performance degradation. Consequently, we propose that to reduce the number of beam measurements (and measurement reporting), RAN2 should introduce height threshold for measurement of a subset of beams. See R2-2211305 [1] for details. |
| LGE | No | We can consider two scenarios:Scenario 1. A Cell quality does not satisfy the report condition, but some beams exceed the threshold of the report condition.Scenario 2. A Cell quality satisfies the report condition, but some beams are weak.In the case of scenario 1, if the target cell is a neighbor cell, the UE will not perform a handover to the corresponding cell. Even if one or two beams are good, if the cell quality is not satisfied, it cannot be considered a good cell. So, the UE does not need to send a measurement report for mobility. If the target cell is a serving cell, the purpose of the measurement report may be beam control. However, the beam can be controlled by the existing procedure such as CSI-RS report. So, the UE does not need to send a measurement report for beam control. In the case of scenario 2, if the cell quality satisfies the report condition, it means that there are beams that satisfy the threshold and can be considered as a good cell. Thus, the weak beams should not affect the measurement report. If the cell quality based on beams (whose beam quantity is higher than absThreshSS-BlocksConsolidation or absThreshCSI-RS-Consolidation) satisfies the report condition, the UE should send the measurement report for mobility.  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

# 3 Conclusions and Proposals

[To be added later by the rapporteur]

# 4 References

[you can add if needed]

[1] R2-2211305, Measurement and reporting enhancements, Qualcomm Incorporated, RAN2#120, Toulouse, France, Nov 14-18, 2022