**3GPP TSG-RAN2 Meeting #121 *R2-230xxxx***

**Athens, Greece, 27th February– 03th March, 2023**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  | **38.306** | **CR** | **0860** | **rev** | **1** | **Current version:** | **17.3.0** |  |
|  |
| *For* [***HELP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network | **X** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Correction on the capability for 1024QAM |
|  |  |
| ***Source to WG:*** | Huawei, HiSilicon |
| ***Source to TSG:*** | RAN2 |
|  |  |
| ***Work item code:*** | NR\_DL1024QAM\_FR1 |  | ***Date:*** | 2023-2-17 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | 1. It is not clear whether the UE shall at most report one of pdsch-1024QAM-2MIMO-FR1-r17and pdsch-1024QAM-FR1-r17.
2. If the UE indicates support of pdsch-1024QAM-2MIMO-FR1-r17, for CC where 1024 QAM is used and it is not clear whether the MIMO layer can be set to more than 2.
3. For reduced 1024QAM capability, the max data rate might not be the data rate calculated by supportedModulationOrderDL in the per CC report.
4. If is not clear whether the legacy scalingFactor and scalingFactor-1024QAM-FR1-r17 can be both included in a FeatureSetPerCC

RAN1 LS R1-2302211 includes:* [4] Assume that Max data rate shall be derived from the higher data rate between 1024 QAM or 256 QAM for CC where 1024 QAM is indicated and the UE support reduced 1024 capability (confirm with R1)

Replies from RAN1: RAN1 confirms the assumption in bullet, which is aligned with the following in TS 38.306 from RAN1’s point of view:*The approximate maximum data rate can be computed as the maximum of the approximate data rates computed using the above formula for each of the supported band or band combinations.** [5] Assume to Clarify that both *scalingFactor* and *scalingFactor-1024QAM-FR1-r17* can be included for in one per CC capability and legacy *scalingFactor* is used when non-1024 QAM is scheduled (confirm with R1)

Replies from RAN1: It’s RAN1’s assumption that both scalingFactor and scalingFactor-1024QAM-FR1-r17 can be included for in one per CC capability and legacy scalingFactor is used when non-1024 QAM is configured. |
|  |  |
| ***Summary of change:*** | 1. Clarfiy that the UE shall at most report one of *pdsch-1024QAM-2MIMO-FR1-r17*and *pdsch-1024QAM-FR1-r17*.
2. Clarfiy that the MIMO layer for 1024 QAM is Min (2, maxNumberMIMO-LayersPDSCH) for the CC where 1024 QAM is reported, and the MIMO layer for non-1024 QAM is *maxNumberMIMO-LayersPDSCH* for UE support *pdsch-1024QAM-2MIMO-FR1-r17*.
3. Clarfiy that max data rate shall be derived from the bigger data rate between 1024 QAM or 256 QAM for CC where 1024 QAM is indicated and the UE support reduced 1024 capability.
4. clarify that both *scalingFactor* and *scalingFactor-1024QAM-FR1-r17* can be included for in one per CC capabltity and legacy *scalingFactor* is used when non-1024 QAM is configured.

**Impact analysis**Impacted 5G architecture options:NR standalone, (NG)EN-DC, NE-DC, NR-DCImpacted functionality:1024QAMInter-operability:1. If the network is implemented according to the CR and the UE is not, the UE supportting *pdsch-1024QAM-2MIMO-FR1-r17* may not report more than 2 MIMO layer for CC supporting 1024 QAM.2. If the UE is implemented according to the CR and the network is not, the UE supportting *pdsch-1024QAM-2MIMO-FR1-r17* may report more than 2 MIMO layers for CC supporting 1024 QAM. The gNB might not understand how this MIMO layer is used. |
|  |  |
| ***Consequences if not approved:*** | 1) Additional *FeatureSet* has to be reported to indicate more than 2 layer MIMO for non-1024 QAM, which will introduce additional signaling load and also may potentially cause RRC reconfiguration when switching transmission for 1024 QAM and non-1024QAM2) Max data rate calcuation might be wrong for CC supporting 1024 QAM with 2 MIMO layer restriction |
|  |  |
| ***Clauses affected:*** | 4.1.2, 4.2.7.2, 4.2.7.5, 4.2.7.6 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **x** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **x** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **x** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

|  |
| --- |
| START OF CHANGE |

## 4.1 Supported max data rate

### 4.1.1 General

The DL, UL and SL max data rate supported by the UE is calculated by band or band combinations supported by the UE. A UE supporting NR (NR SA, MR-DC) shall support the calculated DL and UL max data rate defined in 4.1.2. A UE supporting NR sidelink communication shall support the calculated SL max data rate defined in 4.1.5.

### 4.1.2 Supported max data rate for DL/UL

For NR, the approximate data rate for a given number of aggregated carriers in a band or band combination is computed as follows.



wherein

J is the number of aggregated component carriers in a band or band combination

Rmax = 948/1024

For the j-th CC,

  is the maximum number of supported layers given by higher layer parameter *maxNumberMIMO-LayersPDSCH* for downlink and maximum of higher layer parameters *maxNumberMIMO-LayersCB-PUSCH* and *maxNumberMIMO-LayersNonCB-PUSCH* for uplink.

  is the maximum supported modulation order given by higher layer parameter *supportedModulationOrderDL* for downlink and higher layer parameter *supportedModulationOrderUL* for uplink.

 is the scaling factor given by higher layer parameter *scalingFactor* or *scalingFactor-1024QAM-FR1* and can take the values 1, 0.8, 0.75, and 0.4.

  is the numerology (as defined in TS 38.211 [6])

  is the average OFDM symbol duration in a subframe for numerology , i.e. . Note that normal cyclic prefix is assumed.

  is the maximum RB allocation in bandwidth  with numerology , as defined in 5.3 TS 38.101-1 [2] and 5.3 TS 38.101-2 [3], where  is the UE supported maximum bandwidth in the given band or band combination.

 is the overhead and takes the following values

0.14, for frequency range FR1 for DL

0.18, for frequency range FR2 for DL

0.08, for frequency range FR1 for UL

0.10, for frequency range FR2 for UL

NOTE 1: Only one of the UL or SUL carriers (the one with the higher data rate) is counted for a cell operating SUL.

NOTE 2: For UL Tx switching between carriers, only the supported MIMO layer combination across carriers that results in the highest combined data rate is counted for the carriers in the supported maximum UL data rate.

The approximate maximum data rate can be computed as the maximum of the approximate data rates computed using the above formula for each of the supported band or band combinations. For the CCs where UE supports *pdsch-1024QAM-2MIMO-FR1-r17* for the concerned band, data rate shall be derived as maximum what UE would support if using 1024 QAM (when *mcs-Table-r17* or *mcs-TableDCI-1-2-r17* is configured) or 256 QAM.

For single carrier NR SA operation, the UE shall support a data rate for the carrier that is no smaller than the data rate computed using the above formula, with $J=1 CC$ and component $v\_{Layers}^{(j)}⋅Q\_{m}^{\left(j\right)}⋅f\_{}^{\left(j\right)}$ is no smaller than 4.

NOTE 3: As an example, the value 4 in the component above can correspond to $v\_{Layers}^{(j)}=1$, $Q\_{m}^{\left(j\right)}= 4$ and $f\_{}^{\left(j\right)}=1$.

For EUTRA in case of MR-DC, the approximate data rate for a given number of aggregated carriers in a band or band combination is computed as follows.

Data rate (in Mbps) = $10^{-3}\*\sum\_{j=1}^{J}TBS\_{j  }$

wherein

J is the number of aggregated EUTRA component carriers in MR-DC band combination

$TBS\_{j  }$is the total maximum number of DL-SCH transport block bits received or the total maximum number of UL-SCH transport block bits transmitted, within a 1ms TTI for j-th CC, as derived from TS36.213 [19] based on the UE supported maximum MIMO layers for the j-th CC, and based on the maximum modulation order for the j-th CC and number of PRBs based on the bandwidth of the j-th CC according to indicated UE capabilities.

The approximate maximum data rate can be computed as the maximum of the approximate data rates computed using the above formula for each of the supported band or band combinations.

For MR-DC, the approximate maximum data rate is computed as the sum of the approximate maximum data rates from NR and EUTRA.

*-----------Text omitted-------------*

|  |
| --- |
| NEXT CHANGE |

#### 4.2.7.2 *BandNR parameters*

| Definitions for parameters | Per | M | FDD-TDDDIFF | FR1-FR2DIFF |
| --- | --- | --- | --- | --- |
| ***ack-NACK-FeedbackForMulticastWithDCI-Enabler-r17***Indicates whether the UE supports DCI-based enabling/disabling ACK/NACK based HARQ-ACK feedback configured per G-RNTI by RRC signalling via DCI format 4\_2.A UE supporting this feature shall also indicate support of *ack-NACK-FeedbackForMulticast-r17* and *dynamicMulticastDCI-Format4-2-r17*. | Band | No | N/A | N/A |
| ***ack-NACK-FeedbackForSPS-MulticastWithDCI-Enabler-r17***Indicates whether the UE supports DCI-based enabling/disabling ACK/NACK based HARQ-ACK feedback configured per G-CS-RNTI for multicast by RRC signalling via DCI format 4\_2.A UE supporting this feature shall also indicate support of *ack-NACK-FeedbackForSPS-Multicast-r17*. | Band | No | N/A | N/A |
| ***activeConfiguredGrant-r16***Indicates whether the UE supports up to 12 configured/active configured grant configurations in a BWP of a serving cell. This field includes the following parameters:- *maxNumberConfigsPerBWP-r16* indicates the maximum number of configured/active configured grant configurations in a BWP of a serving cell.- *maxNumberConfigsAllCC-r16* indicates the maximum number of configured/active configured grant configurations across all serving cells in a MAC entity, and across MCG and SCG in case of NR-DC.The UE can include this feature only if the UE indicates support of either *configuredUL-GrantType1* *or configuredUL-GrantType1-v1650* and/or *configuredUL-GrantType2 or configuredUL-GrantType2-v1650*.NOTE:- For all the reported bands in FR1, a same X1 value is reported for *maxNumberConfigsAllCC-r16*. For all the reported bands in FR2, a same X2 value is reported for *maxNumberConfigsAllCC-r16*.- The total number of configured/active configured grant configurations across all serving cells in FR1 is no greater than X1.- The total number of configured/active configured grant configurations across all serving cells in FR2 is no greater than X2.- If the CA have some serving cell(s) in FR1 and some serving cell(s) in FR2, the total number of configured/active configured grant configurations across all serving cells is no greater than max(X1, X2). | Band | No | N/A | N/A |
| ***additionalActiveTCI-StatePDCCH***Indicates whether the UE supports one additional active TCI-State for control in addition to the supported number of active TCI-States for PDSCH. The UE can include this field only if *maxNumberActiveTCI-PerBWP* in *tci-StatePDSCH* is set to *n1*. Otherwise, the UE does not include this field. | Band | No | N/A | N/A |
| ***aperiodicBeamReport***Indicates whether the UE supports aperiodic 'CRI/RSRP' or 'SSBRI/RSRP' reporting on PUSCH. The UE provides the capability for the band number for which the report is provided (where the measurement is performed). | Band | Yes | N/A | N/A |
| ***aperiodicCSI-RS-AdditionalBandwidth-r17***Indicates the UE supported TRS bandwidths for fast SCell activation, in addition to 52 RBs, for a 10MHz UE channel bandwidth. This field only applies for the BWPs configured with 52 RBs size and 15kHz SCS, in FDD bands and indicates the values:Value *addBW-Set1* indicates 28, 32, 36, 40, 44, 48 RBs.Value *addBW-Set2* indicates 32, 36, 40, 44, 48 RBs.The UE can include this feature only if the UE indicates support of *aperiodicCSI-RS-FastScellActivation-r17*. | Band | No | FDD only | FR1 only |
| ***aperiodicCSI-RS-FastScellActivation-r17***Indicates whether the UE supports aperiodic CSI-RS for tracking for fast SCell activation, i.e.,1) Aperiodic CSI-RS for tracking for fast SCell activation is triggered by enhanced SCell activation/deactivation MAC CE;2) Aperiodic CSI-RS for tracking for fast SCell activation is triggered within the BWP indicated by *firstActiveDownlinkBWP-Id* for the SCell.This field includes the following parameters:- *maxNumberAperiodicCSI-RS-PerCC-r17* indicates the maximum number of aperiodic CSI-RS resource set configurations for tracking for fast SCell activation that can be configured to UE per CC in a reported band. Value n8 corresponds to 8, n16 corresponds to 16, and so on.- *maxNumberAperiodicCSI-RS-AcrossCCs-r17* indicates the maximum number of aperiodic CSI-RS resource set configurations for tracking for fast SCell activation that can be configured to UE across CCs in a reported band. Value n8 corresponds to 8, n16 corresponds to 16, and so on.NOTE:- *maxNumberAperiodicCSI-RS-PerCC-r17* and *maxNumberAperiodicCSI-RS-AcrossCCs-r17* values refer to the number of RS configurations for fast SCell activation that can be indicated by the MAC CE.- The NZP-CSI-RS configured as RS for tracking for fast SCell activation are not considered when counting the maximum NZP-CSI-RS configurations of CSI-RS and CSI-IM reception for CSI feedback. | Band | No | N/A | N/A |
| ***aperiodicTRS***Indicates whether the UE supports DCI triggering aperiodic TRS associated with periodic TRS. | Band | No | N/A | Yes |
| ***asymmetricBandwidthCombinationSet***Defines the supported asymmetric channel bandwidth combination for the band as defined in the TS 38.101-1 [2]. Field encoded as a bit map, where bit N is set to "1" if UE support asymmetric channel bandwidth combination set N for this band as defined in the TS 38.101-1 [2]. The leading / leftmost bit (bit 0) corresponds to the asymmetric channel bandwidth combination set 1, the next bit corresponds to the asymmetric channel bandwidth combination set 2 and so on. UE shall support asymmetric channel bandwidth combination set 0. If the field is absent, the UE supports asymmetric channel bandwidth combination set 0. | Band | No | N/A | N/A |
| ***bandNR***Defines supported NR frequency band by NR frequency band number, as specified in TS 38.101-1 [2] and TS 38.101-2 [3]. | Band | Yes | N/A | N/A |
| ***beamCorrespondenceCSI-RS-based-r16***Indicates whether the UE support for beam correspondence based on CSI-RS has the ability to select its uplink beam based on measurement of CSI-RS. If a UE supports beam correspondence based on CSI-RS, then the network can expect the UE to also fulfil Rel-15 beam correspondence requirements.If UE supports neither *beamCorrespondenceSSB-based-r16*nor *beamCorrespondenceCSI-RS-based-r16*, gNB can expect the UE to fulfill beam correspondence based on Rel-15 beam correspondence requirements. | Band | No | TDD only | FR2 only |
| ***beamCorrespondenceSSB-based-r16***Indicates whether the UE support for beam correspondence based on SSB has the ability to select its uplink beam based on measurement of SSB. If a UE supports beam correspondence based on SSB, then the network can expect the UE to also fulfil Rel-15 beam correspondence requirements.If UE supports neither *beamCorrespondenceSSB-based-r16*nor *beamCorrespondenceCSI-RS-based-r16*, gNB can expect the UE to fulfil beam correspondence based on Rel-15 beam correspondence requirements. | Band | No | TDD only | FR2 only |
| ***beamCorrespondenceWithoutUL-BeamSweeping***Indicates how UE supports FR2 beam correspondence as specified in TS 38.101-2 [3], clause 6.6. The UE that fulfils the beam correspondence requirement without the uplink beam sweeping (as specified in TS 38.101-2 [3], clause 6.6) shall set the field to *supported*. The UE that fulfils the beam correspondence requirement with the uplink beam sweeping (as specified in TS 38.101-2 [3], clause 6.6) shall not report this field. | Band | Yes | N/A | FR2 only |
| ***beamManagementSSB-CSI-RS***Defines support of SS/PBCH and CSI-RS based RSRP measurements. The capability comprises signalling of- *maxNumberSSB-CSI-RS-ResourceOneTx* indicates maximum total number of configured one port NZP CSI-RS resources and SS/PBCH blocks that are supported by the UE to measure L1-RSRP as specified in TS 38.215 [13] within a slot and across all serving cells (see NOTE). On FR2, it is mandatory to report >=8; On FR1, it is mandatory with capability signalling to report >=8.- *maxNumberCSI-RS-Resource* indicates maximum total number of configured NZP-CSI-RS resources that are supported by the UE to measure L1-RSRP as specified in TS 38.215 [13] across all serving cells (see NOTE). It is mandated to report at least n8 for FR1.- *maxNumberCSI-RS-ResourceTwoTx* indicates maximum total number of two ports NZP CSI-RS resources that are supported by the UE to measure L1-RSRP as specified in TS 38.215 [13] within a slot and across all serving cells (see NOTE).- *supportedCSI-RS-Density* indicates density of one RE per PRB for one port NZP CSI-RS resource for RSRP reporting, if supported. On FR2, it is mandatory to report either "three" or "oneAndThree"; On FR1, it is mandatory with capability signalling to report either "three" or "oneAndThree".- *maxNumberAperiodicCSI-RS-Resource* indicates maximum number of configured aperiodic CSI-RS resources across all serving cells (see NOTE). For FR1 and FR2, the UE is mandated to report at least n4.NOTE: If the UE sets a value other than *n0* in an FR1 band, it shall set that same value in all FR1 bands. If the UE sets a value other than *n0* in an FR2 band, it shall set that same value in all FR2 bands. The UE supports a total number of resources equal to the maximum of the FR1 and FR2 value, but no more than the FR1 value across all FR1 serving cells and no more than the FR2 value across all FR2 serving cells. | Band | Yes | N/A | FD |
| ***beamReportTiming, beamReportTiming-v1710***Indicates the number of OFDM symbols between the end of the last symbol of SSB/CSI-RS and the start of the first symbol of the transmission channel containing beam report. The UE provides the capability for the band number for which the report is provided (where the measurement is performed). The UE includes this field for each supported sub-carrier spacing. | Band | Yes | N/A | N/A |
| ***beamSwitchTiming, beamSwitchTiming-v1710***Indicates the minimum number of OFDM symbols between the DCI triggering of aperiodic CSI-RS and aperiodic CSI-RS transmission. The number of OFDM symbols is measured from the end of the last symbol containing the indication to the start of the first symbol of CSI-RS. The UE includes this field for each supported sub-carrier spacing.NOTE: *beamSwitchTiming* of value (*sym224* or *sym336* for 60kHz and 120kHz SCS, *sym896* or *sym1344* for 480kHz SCS and *sym1792* or *sym2688* for 960kHz SCS) will be used to determine UE expectation/behaviour for aperiodic CSI-RS for tracking and latency requirements for L1-RSRP reporting as described in clause 5.1.6.1.1 of TS 38.214 [12], while UE behaviour/assumption regarding before or after beam switch timing is unspecified for measuring AP CSI-RS for CSI acquisition (without *trs-Info* and without repetition) and for beam management (with repetition 'off'). | Band | No | N/A | FR2 only |
| ***beamSwitchTiming-r16, beamSwitchTiming-r17***Indicates the minimum number of required OFDM symbols (sym224, sym336 for 60kHz and 120kHz SCS, *sym896* or *sym1344* for 480kHz SCS and *sym1792* or *sym2688* for 960kHz SCS) between the DCI triggering aperiodic CSI-RS and the corresponding aperiodic CSI-RS transmission in a CSI-RS resource set configured with repetition 'ON' if *enableBeamSwitchTiming-r16* is configured.For CSI-RS configured with repetition "*off*", the UE applies beam switch time of sym48 if *beamSwitchTiming-r16* is reported and *enableBeamSwitchTiming-r16* is configured. For CSI-RS configured without repetition and without *trs-info*, the UE applies beam switch time of sym48 if *beamSwitchTiming-r16* is reported and *enableBeamSwitchTiming-r16* is configured. | Band | No | N/A | FR2 only |
| ***bfd-Relaxation-r17***Indicates whether the UE supports BFD relaxation criteria and requirement as specified in TS 38.133 [5]. UE shall set the capability value consistently for all FDD-FR1 bands, all TDD-FR1 bands, all TDD-FR2-1 bands and all TDD-FR2-2 bands respectively.UE indicating support of this feature shall also indicate support of *maxNumberCSI-RS-BFD, maxNumberSSB-BFD* and *maxNumberCSI-RS-SSB-CBD.* | Band  | No | N/A | N/A |
| ***bwp-DiffNumerology***Indicates whether the UE supports BWP adaptation up to 4 BWPs with the different numerologies, via DCI and timer. Except for SUL, the UE only supports the same numerology for the active UL and DL BWP. For the UE capable of this feature, the bandwidth of a UE-specific RRC configured DL BWP includes the bandwidth of the CORESET#0 (if CORESET#0 is present) and SSB for PCell and PSCell (if configured). For SCell(s), the bandwidth of the UE-specific RRC configured DL BWP includes SSB, if there is SSB on SCell(s). | Band | No | N/A | N/A |
| ***bwp-SameNumerology***Indicates whether UE supports BWP adaptation (up to 2/4 BWPs) with the same numerology, via DCI and timer. Except for SUL, the UE only supports the same numerology for the active UL and DL BWP. For the UE capable of this feature, the bandwidth of a UE-specific RRC configured DL BWP includes the bandwidth of the CORESET#0 (if CORESET#0 is present) and SSB for PCell and PSCell (if configured). For SCell(s), the bandwidth of the UE-specific RRC configured DL BWP includes SSB, if there is SSB on SCell(s). | Band | No | N/A | N/A |
| ***bwp-WithoutRestriction***Indicates support of BWP operation without bandwidth restriction. The Bandwidth restriction in terms of DL BWP for PCell and PSCell means that the bandwidth of a UE-specific RRC configured DL BWP may not include the bandwidth of CORESET #0 (if configured) and SSB. For SCell(s), it means that the bandwidth of DL BWP may not include SSB. | Band | No | N/A | N/A |
| ***cancelOverlappingPUSCH-r16***Indicates whether UE supports the cancellation of the (repetition of the) PUSCHs transmission on all other intra-band serving cell(s). The cancellation of the (repetition of the) PUSCH transmission on a the set of intra-band serving cell(s) includes all symbols from the earliest symbol that is overlapping with the first cancelled symbol of the PUSCH on the serving cell for which the DCI format 2\_4 is applicable to. If the UE supports this feature, the UE needs to report *pa-PhaseDiscontinuityImpacts* and *ul-CancellationSelfCarrier-r16*. | Band | No | N/A | N/A |
| ***cg-SDT-r17***Indicates whether the UE supports transmission of data and/or signalling over allowed radio bearers in RRC\_INACTIVE state via configured grant type 1 (i.e. CG-SDT), as specified in TS 38.331 [9]. Except for NTN bands, UE shall set the capability value consistently for all FDD-FR1 bands, all TDD-FR1 bands and all TDD-FR2 bands respectively. For NTN, UE shall set the capability value consistently for all FDD-FR1 NTN bands.UE supports multiple CG-SDT configurations when a UE indicates the support of this feature and *activeConfiguredGrant-r16*; otherwise UE only supports one CG-SDT configuration. | Band | No | N/A | N/A |
| ***channelBWs-DL***Indicates for each subcarrier spacing the UE supported channel bandwidths.Absence of the *channelBWs-DL* (without suffix) for a band or absence of specific scs-XXkHz entry for a supported subcarrier spacing means that the UE supports the channel bandwidths among [5, 10, 15, 20, 25, 30, 40, 50, 60, 80, 100] and [50, 100, 200] that were defined in clause 5.3.5 of TS 38.101-1 version 15.7.0 [2] and TS 38.101-2 version 15.7.0 [3] for the given band or the specific SCS entry. For IAB-MT, to determine whether the IAB-MT supports a channel bandwidth of 100 MHz, the network checks c*hannelBW-DL-IAB-r16*.For FR1, the bits in *channelBWs-DL* (without suffix) starting from the leading / leftmost bit indicate 5, 10, 15, 20, 25, 30, 40, 50, 60 and 80MHz. For FR2, the bits in *channelBWs-DL* (without suffix) starting from the leading / leftmost bit indicate 50, 100 and 200MHz. The third / rightmost bit (for 200MHz) shall be set to 1. For IAB-MT the third / rightmost bit (for 200MHz) is ignored. To determine whether the IAB-MT supports a channel bandwidth of 200 MHz, the network checks *channelBW-DL-IAB-r16*.For FR1, the leading/leftmost bit in *channelBWs-DL-v1590* indicates 70MHz, the second leftmost bit indicates 45MHz, the third leftmost bit indicates 35MHz, the fourth leftmost bit indicates 100MHz and all the remaining bits in *channelBWs-DL-v1590* shall be set to 0. The fourth leftmost bit (for 100MHz) is not applicable for bands n41, n48, n77, n78, n79 and n90 as defined in TS 38.101-1 [2]. For each band, RedCap UEs shall indicate supporting the maximum of those channel bandwidths that are less than or equal to 20 MHz for FR1 and less than or equal to 100 Mhz for FR2, taking restrictions in TS 38.101-1 [2] and TS 38.101-2 [3] into consideration.This feature is applicable only for FR1 and FR2-1 band, otherwise it is absent.NOTE: To determine whether the UE supports a specific SCS for a given band, the network validates the *supportedSubCarrierSpacingDL* and the *scs-60kHz*.To determine whether the UE supports a channel bandwidth of 90 MHz, the network may ignore this capability and validate instead the *channelBW-90mhz*, the *supportedBandwidthCombinationSet* and the *supportedBandwidthCombinationSetIntraENDC*. To determine whether the UE supports a channel bandwidth of 400 MHz, the network may ignore this capability and validate the *supportedBandwidthCombinationSet*, the *supportedBandwidthCombinationSetIntraENDC*, and the *supportedBandwidthDL*. For serving cell(s) with other channel bandwidths the network validates the *channelBWs-DL*, the *supportedBandwidthCombinationSet*, the *supportedBandwidthCombinationSetIntraENDC*, the *asymmetricBandwidthCombinationSet* (for a band supporting asymmetric channel bandwidth as defined in clause 5.3.6 of TS 38.101-1 [2]), *supportedBandwidthDL* and *supportedMinBandwidthDL*.. | Band | Yes | N/A | N/A |
| ***channelBWs-DL-SCS-120kHz-FR2-2-r17***Indicates the UE supported channel bandwidths in DL for the SCS 120kHz.The bits in *channelBWs-DL-SCS-120kHz-FR2-2* starting from the leading / leftmost bit indicate 100 and 400MHz.100 and 400 MHz are mandatory channel bandwidths if the UE supports 120 kHz SCS (i.e. the bit for 100 and 400MHz shall always be set to 1).UE supporting this feature shall also indicate support of *dl-FR2-2-SCS-120kHz-r17*.NOTE: To determine whether the UE supports a SCS 120kHz for a given band, the network validates the *supportedSubCarrierSpacingDL*.To determine the supported carrier bandwidths, the network validates the *channelBWs-DL-SCS-120kHz-FR2-2-r17*, the *supportedBandwidthCombinationSet* and the *supportedBandwidthDL-v1710*. | Band | CY | N/A | N/A |
| ***channelBWs-DL-SCS-480kHz-FR2-2-r17***Indicates the UE supported channel bandwidths in DL for the SCS 480kHz.The bits in *channelBWs-DL-SCS-480kHz-FR2-2* starting from the leading / leftmost bit indicate 400, 800 and 1600MHz.400 MHz is a mandatory channel bandwidth if the UE supports 480 kHz SCS (i.e. the bit for 400MHz shall always be set to 1).UE supporting this feature shall also indicate support of *dl-FR2-2-SCS-480kHz-r17*.NOTE: To determine whether the UE supports a SCS 480kHz for a given band, the network validates the *supportedSubCarrierSpacingDL*.To determine the supported carrier bandwidths, the network validates the *channelBWs-DL-SCS-480kHz-FR2-2-r17*, the *supportedBandwidthCombinationSet* and *supportedBandwidthDL-v1710*. | Band | CY | N/A | N/A |
| ***channelBWs-DL-SCS-960kHz-FR2-2-r17***Indicates the UE supported channel bandwidths in DL for the SCS 960kHz.The bits in *channelBWs-DL-SCS-960kHz-FR2-2* starting from the leading / leftmost bit indicate 400, 800,1600 and 2000MHz.400 MHz is a mandatory channel bandwidth if the UE supports 960 kHz SCS (i.e. the bit for 400MHz shall always be set to 1).UE supporting this feature shall also indicate support of *dl-FR2-2-SCS-960kHz-r17*.NOTE: To determine whether the UE supports a SCS 960kHz for a given band, the network validates the *supportedSubCarrierSpacingDL*.To determine the supported carrier bandwidths, the network validates the *channelBWs-DL-SCS-960kHz-FR2-2-r17*, the *supportedBandwidthCombinationSet* and *supportedBandwidthDL-v1710*. | Band | CY | N/A | N/A |
| ***channelBWs-UL***Indicates for each subcarrier spacing the UE supported channel bandwidths.Absence of the *channelBWs-UL* (without suffix) for a band or absence of specific scs-XXkHz entry for a supported subcarrier spacing means that the UE supports the channel bandwidths among [5, 10, 15, 20, 25, 30, 40, 50, 60, 80, 100] and [50, 100, 200] that were defined in clause 5.3.5 of TS 38.101-1 version 15.7.0 [2] and TS 38.101-2 version 15.7.0 [3] for the given band or the specific SCS entry. For IAB-MT, to determine whether the IAB-MT supports a channel bandwidth of 100 MHz, the network checks *channelBW-UL-IAB-r16*.For FR1, the bits in *channelBWs-UL* (without suffix) starting from the leading / leftmost bit indicate 5, 10, 15, 20, 25, 30, 40, 50, 60 and 80MHz. For FR2, the bits in *channelBWs-UL* (without suffix) starting from the leading / leftmost bit indicate 50, 100 and 200MHz. The third / rightmost bit (for 200MHz) shall be set to 1. For IAB-MT the third / rightmost bit (for 200MHz) is ignored. To determine whether the IAB-MT supports a channel bandwidth of 200 MHz, the network checks *channelBW-UL-IAB-r16*.For FR1, the leading/leftmost bit in *channelBWs-UL-v1590* indicates 70 MHz, the second leftmost bit indicates 45MHz, the third leftmost bit indicates 35MHz, the fourth leftmost bit indicates 100MHz and all the remaining bits in *channelBWs-UL-v1590* shall be set to 0. The fourth leftmost bit (for 100MHz) is not applicable for bands n41, n48, n77, n78, n79 and n90 as defined in TS 38.101-1 [2]. For each band, RedCap UEs shall indicate supporting the maximum of those channel bandwidths that are less than or equal to 20 MHz for FR1 and less than or equal to 100 Mhz for FR2, taking restrictions in TS 38.101-1 [2] and TS 38.101-2 [3] into consideration.This feature is applicable only for FR1 and FR2-1 band, otherwise it is absent.NOTE: To determine whether the UE supports a specific SCS for a given band, the network validates the *supportedSubCarrierSpacingUL* and the *scs-60kHz*.To determine whether the UE supports a channel bandwidth of 90 MHz the network may ignore this capability and validate instead the *channelBW-90mhz*, the *supportedBandwidthCombinationSet* and the *supportedBandwidthCombinationSetIntraENDC*. To determine whether the UE supports a channel bandwidth of 400 MHz, the network may ignore this capability and validate the *supportedBandwidthCombinationSet*, the *supportedBandwidthCombinationSetIntraENDC*, and the *supportedBandwidthUL*. For serving cell(s) with other channel bandwidths the network validates the *channelBWs-UL*, the *supportedBandwidthCombinationSet*, the *supportedBandwidthCombinationSetIntraENDC*, the *asymmetricBandwidthCombinationSet* (for a band supporting asymmetric channel bandwidth as defined in clause 5.3.6 of TS 38.101-1 [2]), *supportedBandwidthUL* and *supportedMinBandwidthUL*. | Band | Yes | N/A | N/A |
| ***channelBWs-UL-SCS-120kHz-FR2-2-r17***Indicates the UE supported channel bandwidths in UL for the SCS 120kHz.The bits in *channelBWs-UL-SCS-120kHz-FR2-2* starting from the leading / leftmost bit indicate 100 and 400MHz.100 and 400 MHz are mandatory channel bandwidths if the UE supports 120 kHz SCS (i.e. the bit for 100 and 400MHz shall always be set to 1).UE supporting this feature shall also indicate support of *ul-FR2-2-SCS-120kHz-r17*.NOTE: To determine whether the UE supports a SCS 120kHz for a given band, the network validates the *supportedSubCarrierSpacingUL*.To determine the supported carrier bandwidths, the network validates the *channelBWs-UL-SCS-120kHz-FR2-2-r17*, the *supportedBandwidthCombinationSet* and the *supportedBandwidthUL-v1710*. | Band | CY | N/A | N/A |
| ***channelBWs-UL-SCS-480kHz-FR2-2-r17***Indicates the UE supported channel bandwidths in UL for the SCS 480kHz.The bits in *channelBWs-UL-SCS-480kHz-FR2-2* starting from the leading / leftmost bit indicate 400, 800 and 1600MHz.400 MHz is a mandatory channel bandwidth if the UE supports 480 kHz SCS (i.e. the bit for 400MHz shall always be set to 1).UE supporting this feature shall also indicate support of *ul-FR2-2-SCS-480kHz-r17*.NOTE: To determine whether the UE supports a SCS 480kHz for a given band, the network validates the *supportedSubCarrierSpacingUL*.To determine the supported carrier bandwidths, the network validates the *channelBWs-UL-SCS-480kHz-FR2-2-r17*, the *supportedBandwidthCombinationSet* and *supportedBandwidthUL-v1710*. | Band | CY | N/A | N/A |
| ***channelBWs-UL-SCS-960kHz-FR2-2-r17***Indicates the UE supported channel bandwidths in UL for the SCS 960kHz.The bits in *channelBWs-UL-SCS-960kHz-FR2-2* starting from the leading / leftmost bit indicate 400, 800, 1600 and 2000MHz.400 MHz is a mandatory channel bandwidth if the UE supports 960 kHz SCS (i.e. the bit for 400MHz shall always be set to 1).UE supporting this feature shall also indicate support of *ul-FR2-2-SCS-960kHz-r17*.NOTE: To determine whether the UE supports a SCS 960kHz for a given band, the network validates the *supportedSubCarrierSpacingUL*.To determine the supported carrier bandwidths, the network validates the *channelBWs-UL-SCS-960kHz-FR2-2-r17*, the *supportedBandwidthCombinationSet* and *supportedBandwidthUL-v1710*. | Band | CY | N/A | N/A |
| ***channelBW-DL-IAB-r16***Indicates whether the IAB-MT supports channel bandwidth of 100 MHz for a given SCS in FR1 for DL or whether the IAB-MT supports channel bandwidth of 200 MHz for a given SCS in FR2 for DL. | Band | No | N/A | N/A |
| ***channelBW-UL-IAB-r16***Indicates whether the IAB-MT supports channel bandwidth of 100 MHz for a given SCS in FR1 for UL or whether the IAB-MT supports channel bandwidth of 200 MHz for a given SCS in FR2 for UL. | Band | No | N/A | N/A |
| ***codebookComboParametersAddition-r16***Indicates the UE supports the mixed codebook combinations and the corresponding parameters supported by the UE.For mixed codebook types, UE reports support active CSI-RS resources and ports for up to 4 mixed codebook combinations in any slot. The following is the possible mixed codebook combinations:- {Type 1 Single Panel, Type 2, Null}- {Type 1 Single Panel, Type 2 with port selection, Null}- {Type 1 Single Panel, eType 2 with R=1, Null}- {Type 1 Single Panel, eType 2 with R=2, Null}- {Type 1 Single Panel, eType 2 with R=1 and port selection, Null}- {Type 1 Single Panel, eType 2 with R=2 and port selection, Null}- {Type 1 Single Panel, Type 2, Type 2 with port selection}- {Type 1 Multi Panel, Type 2, Null}- {Type 1 Multi Panel, Type 2 with port selection, Null}- {Type 1 Multi Panel, eType 2 with R=1, Null}- {Type 1 Multi Panel, eType 2 with R=2, Null}- {Type 1 Multi Panel, eType 2 with R=1 with port selection, Null}- {Type 1 Multi Panel, eType 2 with R=2 with port selection, Null}- {Type 1 Multi Panel, Type 2, Type 2 with port selection}Parameters for each mixed codebook supported by the UE:- *supportedCSI-RS-ResourceListAdd-r16* indicates the list of supported CSI-RS resources in a band by referring to *codebookVariantsList*. The following parameters are included in *codebookVariantsList*:For *supportedCSI-RS-ResourceListAdd-r16* related to the additional codebooks:- The minimum of *maxNumberTxPortsPerResource* is '*p4*';- The minimum value of *totalNumberTxPortsPerBand* is 4.If a UE reports one or more mixed codebook combinations, then usage of active CSI-RS resources and ports for multiple codebooks in any slot is allowed only within those combinations. For coexisting of mixed codebooks in any slot, gNB needs to consider the mixed codebook combination capability as well as per codebook capability of each codebook type in the mixed codebook combination.UE indicates support of a codebook type in the mixed codebook combination shall indicates support of the individual codebook type in the per band capability. | Band | No | N/A | N/A |
| ***codebookParameters***Indicates the codebooks and the corresponding parameters supported by the UE.Parameters for type I single panel codebook (type1 singlePanel) supported by the UE, which are mandatory to report:- *supportedCSI-RS-ResourceList*;- a UE shall support a *maxNumberTxPortsPerResource* minimum value of 4 for codebook type I single panel in FR1 in the case of a single active CSI-resource across all bands in a band combination, regardless of what it reports in *supportedCSI-RS-ResourceList* with *maxNumberTxPortsPerResource*;- a UE shall support a *maxNumberTxPortsPerResource* minimum value of 8 when configured with wideband CSI report for codebook type I single panel in FR1 in the case of a single active CSI-resource across all bands in a band combination, regardless of what it reports in *supportedCSI-RS-ResourceList* with *maxNumberTxPortsPerResource*;- a UE shall support a *maxNumberTxPortsPerResource* minimum value of 2 for codebook type I single panel in FR2 in the case of a single active CSI-resource across all bands in a band combination, regardless of what it reports in *supportedCSI-RS-ResourceList* with *maxNumberTxPortsPerResource*.- *modes* indicates supported codebook modes (mode 1, both mode 1 and mode 2);- *maxNumberCSI-RS-PerResourceSet* indicates the maximum number of CSI-RS resource in a resource set.Parameters for type I multi-panel codebook (type1 multiPanel) supported by the UE, which are optional:- *supportedCSI-RS-ResourceList*;- *modes* indicates supported codebook modes (mode 1, mode 2, or both mode 1 and mode 2);- *maxNumberCSI-RS-PerResourceSet* indicates the maximum number of CSI-RS resource in a resource set;- *nrofPanels* indicates supported number of panels.Parameters for type II codebook (type2) supported by the UE, which are optional:- *supportedCSI-RS-ResourceList*;- *parameterLx* indicates the parameter "Lx" in codebook generation where x is an index of Tx ports indicated by *maxNumberTxPortsPerResource*;- *amplitudeScalingType* indicates the amplitude scaling type supported by the UE (wideband or both wideband and sub-band);- *amplitudeSubsetRestriction* indicates whether amplitude subset restriction is supported for the UE.Parameters for type II codebook with port selection (type2-PortSelection) supported by the UE, which are optional:- *supportedCSI-RS-ResourceList*;- *parameterLx* indicates the parameter "Lx" in codebook generation where x is an index of Tx ports indicated by *maxNumberTxPortsPerResource*;- *amplitudeScalingType* indicates the amplitude scaling type supported by the UE (wideband or both wideband and sub-band).*supportedCSI-RS-ResourceList* includes list of the following parameters:- *maxNumberTxPortsPerResource* indicates the maximum number of Tx ports in a resource;- *maxNumberResourcesPerBand* indicates the maximum number of resources across all CCs within a band simultaneously;- *totalNumberTxPortsPerBand* indicates the total number of Tx ports across all CCs within a band simultaneously.For each codebook type, the UE may report another list of supported CSI-RS resources via *supportedCSI-RS-ResourceListAlt* in *codebookParametersPerBand*. For type I single panel codebook (type1 singlePanel) supportedCSI-RS-ResourceListAlt,- a UE shall report at least one triplet in supportedCSI-RS-ResourceListAlt with maxNumberTxPortsPerResource greater than or equal to 8 for FR1;- a UE shall report at least one triplet in supportedCSI-RS-ResourceListAlt with maxNumberTxPortsPerResource greater than or equal to 2 for FR2. | Band | FD | N/A | N/A |
| ***codebookParametersAddition-r16***Indicates the UE support of additional codebooks and the corresponding parameters supported by the UE.Codebook etype 2 R=1 support parameter combination 1 to 6 and rank 1 to 2. Parameters for etype 2 R=1 (*etype2R1-r16*) supported by the UE, which are optional:- *supportedCSI-RS-ResourceListAdd-r16* indicates the list of supported CSI-RS resources in a band by referring to *codebookVariantsList*. The following parameters are included in *codebookVariantsList*:- *maxNumberTxPortsPerResource* indicates the maximum number of Tx ports in a resource of a band;- *maxNumberResourcesPerBand* indicates the maximum number of resources across all CCs in a band, simultaneously;- *totalNumberTxPortsPerBand* indicates the total number of Tx ports across all CCs in a band, simultaneously.- *paramComb7-8-r16* indicates the support of parameter combinations 7-8 for etype 2 R=1- *rank3-4-r16* indicates the support of rank 3,4.- *amplitudeSubsetRestriction-r16* indicates the support of amplitude subset restriction.Parameters for etype 2 R=2 (*etype2R2-r16*) supported by the UE, which are optional:- *supportedCSI-RS-ResourceListAdd-r16*;UE supporting *etype2R2-r16*supports also indicates support of *etype2R1-r16*.Codebook etype 2 R=1 with port selection supports 6 parameter combinations and rank 1,2. Parameters for etype 2 R=1 with port selection (*etype2R1-PortSelection-r16*) supported by the UE, which are optional:- *supportedCSI-RS-ResourceListAdd-r16*;- *rank3-4-r16* indicates the support of rank 3,4Parameters for etype 2 R=2 with port selection (*etype2R2-PortSelection-r16*) supported by the UE, which are optional:- *supportedCSI-RS-ResourceListAdd-r16*;UE supporting *etype2R2-PortSelection-r16* also indicates support of *etype2R1-PortSelection-r16*.For *supportedCSI-RS-ResourceListAdd-r16* related to the additional codebooks:- The minimum of *maxNumberTxPortsPerResource* is '*p4*';- The minimum value of *totalNumberTxPortsPerBand* is 4. | Band | No | N/A | N/A |
| ***codebookParametersfetype2-r17***Indicates the UE support of additional codebooks and the corresponding parameters supported by the UE of Further Enhanced Port-Selection Type II Codebook (FeType-II).The UE indicating this feature shall include *fetype2basic-r17* to indicate basic features of FeType-II. This capability signalling comprises the following parameters:*-* indicates the list of supported CSI-RS resources in a band by referring to *codebookVariantsList*. The following parameters are included in *codebookVariantsList*:- *maxNumberTxPortsPerResource* indicates the maximum number of Tx ports in a resource of a band- *maxNumberResourcesPerBand* indicates the maximum number of resources across all CCs in a band, simultaneously- *totalNumberTxPortsPerBand* indicates the total number of Tx ports across all CCs in a band, simultaneouslyThe UE indicating *fetype2basic-r17* shall support parameter combinations with M=1 and support rank 1 and 2. UE indicating this feature shall also include *csi-ReportFramework*.The UE optionally includes *fetype2R1-r17* to indicate whether the UE supports M=2 and R=1 for FeType-II. This capability signalling comprises the following parameters:*-* indicates the list of supported CSI-RS resources in a band by referring to *codebookVariantsList*.The UE indicating support of *fetype2R1-r17* shall also indicate support of *fetype2basic-r17* and parameter combinations with M=2.The UE optionally includes *fetype2R2-r17* to indicate whether the UE supports rank = 2 for FeType-II. This capability signalling comprises the following parameters:*-* indicates the list of supported CSI-RS resources in a band by referring to *codebookVariantsList*.UE indicating support of *fetype2R2-r17* shall also indicate support of *fetype2R1-r17*.The UE optionally includes *fetype2Rank3Rank4-r17* to indicate whether the UE supports rank = 3 and rank = 4 for FeType-II. UE indicating support of *fetype2Rank3Rank4-r17* shall indicate support of *fetype2basic-r17*.For *codebookVariantsList* related to the FeType-II:- The minimum of *maxNumberTxPortsPerResource* is '*p4*';- The minimum value of *totalNumberTxPortsPerBand* is 4. | Band | No | N/A | N/A |
| ***codebookComboParameterMixedType-r17***Indicates the support of active CSI-RS resources and ports for mixed codebook types in any slot. The UE reports support active CSI-RS resources and ports for up to 4 mixed codebook combinations in any slot. The following are the possible mixed codebook combinations {Codebook1, Codebook2, Codebook3}:*- type1SP-feType2PS-null-r17 indicates* {Type 1 Single Panel, FeType II PS M=1, NULL}*- type1SP-feType2PS-M2R1-null-r17* indicates {Type 1 Single Panel, FeType II PS M=2 R=1, NULL}*- type1SP-feType2PS-M2R2-null-r17* indicates {Type 1 Single Panel, FeType II PS M=2 R=2, NULL}*- type1SP-Type2-feType2-PS-M1-r17* indicates {Type 1 Single Panel, Type II, FeType II PS M=1}*- type1SP-Type2-feType2-PS-M2R1-r17* indicates {Type 1 Single Panel, Type II, FeType II PS M=2 R=1}*-* *type1SP-eType2R1-feType2-PS-M1-r17* indicates {Type 1 Single Panel, eType II R=1, FeType II PS M=1}*-* *type1SP-eType2R1-feType2-PS-M2R1-r17* indicates {Type 1 Single Panel, eType II R=1, FeType II PS M=2 R=1}*-* *type1MP-feType2PS-null-r17* indicates {Type 1 Multi Panel*,* FeType II PS M=1, NULL}*-* *type1MP-feType2PS-M2R1-null-r17* indicates {Type 1 Multi Panel*,* FeType II PS M=2 R=1, NULL}*-* *type1MP-feType2PS-M2R2-null-r17* indicates {Type 1 Multi Panel*,* FeType II PS M=2 R=2, NULL}*-* *type1MP-Type2-feType2-PS-M1-r17* indicates {Type 1 Multi Panel*,* Type II, FeType II PS M=1}*-* *type1MP-Type2-feType2-PS-M2R1-r17* indicates {Type 1 Multi Panel*,* Type II, FeType II PS M=2 R=1}*-* *type1MP-eType2R1-feType2-PS-M1-r17* indicates {Type 1 Multi Panel, eType II R=1, FeType II PS M=1}*-* *type1MP-eType2R1-feType2-PS-M2R1-r17* indicates {Type 1 Multi Panel*,* eType II R=1, FeType II PS M=2 R=1}For each mixed codebook supported by the UE, *supportedCSI-RS-ResourceListAdd-r16* indicates the list of supported CSI-RS resources in a band by referring to *codebookVariantsList*. The following parameters are included for the supported CSI-RS resource:*-* *maxNumberTxPortsPerResource* indicates the maximum number of Tx ports in a resource of a band. The minimum of *maxNumberTxPortsPerResource* is 'p4';- *maxNumberResourcesPerBand* indicates the maximum number of resources across all CCs in a band;- *totalNumberTxPortsPerBand* indicates the total number of Tx ports across all CCs in a band. The minimum value of *totalNumberTxPortsPerBand* is 4.The UE supporting this feature shall indicate the support of *fetype2basic-r17, etype2R1-r16, CodebookComboParametersAddition-r16, supportedCSI-RS-ResourceList, fetype2R1-r17, fetype2R2-r17.* | Band | No | N/A | N/A |
| ***codebookComboParameterMultiTRP-r17***Indicates the support of active CSI-RS resources and ports in the presence of multi-TRP CSI.Indicates the support of active CSI-RS resources and ports for mixed codebook types in any slot. The UE reports supported active CSI-RS resources and ports for up to 4 mixed codebook combinations. The following are the possible mixed codebook combinations {Codebook1, Codebook2, Codebook3}:*-* *nCJT-null-null* indicates {NCJT, NULL, NULL}*-* *nCJT1SP-null-null* indicates {NCJT+Type 1 SP for sTRP, NULL, NULL}*- nCJT-Type2-null-r16* indicates{NCJT*, Type 2, Null*}*- nCJT-Type2PS-null-r16* indicates{NCJT*, Type 2 with port selection, Null*}*- nCJT-eType2R1-null-r16* indicates{NCJT*, eType 2 with R=1, Null*}*- nCJT-eType2R2-null-r16* indicates {NCJT*, eType 2 with R=2, Null*}*- nCJT-eType2R1PS-null-r16* indicates {NCJT*, eType 2 with R=1 and port selection, Null*}*- nCJT-eType2R2PS-null-r16* indicates {NCJT*, eType 2 with R=2 and port selection, Null*}*- nCJT-Type2-Type2PS-r16* indicates {NCJT*, Type 2, Type 2 with port selection*}*- nCJT1SP-Type2-null-r16* indicates{NCJT+Type 1 SP for sTRP, Type 2, Null}*- nCJT1SP-Type2PS-null-r16* indicates{NCJT+Type 1 SP for sTRP, Type 2 with port selection, Null}*- nCJT1SP-eType2R1-null-r16* indicates{NCJT+Type 1 SP for sTRP, eType 2 with R=1, Null}*- nCJT1SP-eType2R2-null-r16* indicates{NCJT+Type 1 SP for sTRP, eType 2 with R=2, Null}*- nCJT1SP-eType2R1PS-null-r16* indicates{NCJT+Type 1 SP for sTRP, eType 2 with R=1 and port selection, Null}*- nCJT1SP-eType2R2PS-null-r16* indicates{NCJT+Type 1 SP for sTRP, eType 2 with R=2 and port selection, Null}*- nCJT1SP-Type2-Type2PS-r16* indicates{NCJT+Type 1 SP for sTRP, Type 2, Type 2 with port selection}*- nCJT-feType2PS-null-r17 indicates* {NCJT, FeType II PS M=1, NULL}*- nCJT-feType2PS-M2R1-null-r17* indicates {NCJT, FeType II PS M=2 R=1, NULL}*- nCJT-feType2PS-M2R2-null-r17* indicates {NCJT, FeType II PS M=2 R=2, NULL}*- nCJT-Type2-feType2-PS-M1-r17* indicates {NCJT, Type II, FeType II PS M=1}*- nCJT-Type2-feType2-PS-M2R1-r17* indicates {NCJT, Type II, FeType II PS M=2 R=1}*-* *nCJT-eType2R1-feType2-PS-M1-r17* indicates {NCJT, eType II R=1, FeType II PS M=1}*-* *nCJT-eType2R1-feType2-PS-M2R1-r17* indicates {NCJT, eType II R=1, FeType II PS M=2 R=1}*- nCJT1SP-feType2PS-null-r17 indicates* {NCJT+Type 1 SP for sTRP, FeType II PS M=1, NULL}*- nCJT1SP-feType2PS-M2R1-null-r17* indicates {NCJT+Type 1 SP for sTRP, FeType II PS M=2 R=1, NULL}*- nCJT1SP-feType2PS-M2R2-null-r17* indicates {NCJT+Type 1 SP for sTRP, FeType II PS M=2 R=2, NULL}*- nCJT1SP-Type2-feType2-PS-M1-r17* indicates {NCJT+Type 1 SP for sTRP, Type II, FeType II PS M=1}*- nCJT1SP-Type2-feType2-PS-M2R1-r17* indicates {NCJT+Type 1 SP for sTRP, Type II, FeType II PS M=2 R=1}*-* *nCJT1SP-eType2R1-feType2-PS-M1-r17* indicates {NCJT+Type 1 SP for sTRP, eType II R=1, FeType II PS M=1}*-* *nCJT1SP-eType2R1-feType2-PS-M2R1-r17* indicates {NCJT+Type 1 SP for sTRP, eType II R=1, FeType II PS M=2 R=1}For each mixed codebook supported by the UE, *supportedCSI-RS-ResourceListAdd-r16* indicates the list of supported CSI-RS resources in a band by referring to *codebookVariantsList*. The following parameters are included in *codebookVariantsList*:*-* *maxNumberTxPortsPerResource* indicates the maximum number of Tx ports in a resource of a band combination.- *maxNumberResourcesPerBand* indicates the maximum number of resources across all CCs in a band combination.- *totalNumberTxPortsPerBand* indicates the total number of Tx ports across all CCs in a band combination.NOTE 1: A CMR pair configured for NCJT will be counted as two activated resources, a CMR configured for sTRP will be counted as one activated resource for a triplet.NOTE 2: This capability is relevant only when UE is configured with NCJT CSI in at least one CSI report setting in at least one CC in the band and/or band combination.The UE indicating support of this feature shall also indicate the support of *mTRP-CSI-EnhancementPerBand-r17*. | Band | No | N/A | N/A |
| ***condHandover-r16***Indicates whether the UE supports conditional handover including execution condition, candidate cell configuration and maximum 8 candidate cells. Except for NTN bands, UE shall set the capability value consistently for all FDD-FR1 bands, all TDD-FR1 bands, all TDD-FR2-1 bands and all TDD-FR2-2 bands respectively. For NTN, UE shall set the capability value consistently for all FDD-FR1 NTN bands. | Band | No | N/A | N/A |
| ***condHandoverFailure-r16***Indicates whether the UE supports conditional handover during re-establishment procedure when the selected cell is configured as candidate cell for condition handover. Except for NTN bands, UE shall set the capability value consistently for all FDD-FR1 bands, all TDD-FR1 bands, all TDD-FR2-1 bands and all TDD-FR2-2 bands respectively. For NTN, UE shall set the capability value consistently for all FDD-FR1 NTN bands. | Band | No | N/A | N/A |
| ***condHandoverTwoTriggerEvents-r16***Indicates whether the UE supports 2 trigger events for same execution condition. This feature is mandatory supported if the UE supports *condHandover-r16*. Except for NTN bands, UE shall set the capability value consistently for all FDD-FR1 bands, all TDD-FR1 bands, all TDD-FR2-1 bands and all TDD-FR2-2 bands respectively. For NTN, UE shall set the capability value consistently for all FDD-FR1 NTN bands. | Band | CY | N/A | N/A |
| ***condPSCellChange-r16***Indicates whether the UE supports conditional PSCell change including execution condition, candidate cell configuration and maximum 8 candidate cells. UE shall set the capability value consistently for all FDD-FR1 bands, all TDD-FR1 bands, all TDD-FR2-1 bands and all TDD-FR2-2 bands respectively. | Band | No | N/A | N/A |
| ***condPSCellChangeTwoTriggerEvents-r16***Indicates whether the UE supports 2 trigger events for same execution condition. This feature is mandatory supported if the UE supports *condPSCellChange-r16*. UE shall set the capability value consistently for all FDD-FR1 bands, all TDD-FR1 bands, all TDD-FR2-1 bands and all TDD-FR2-2 bands respectively. | Band | CY | N/A | N/A |
| ***configuredUL-GrantType1-v1650***Indicates whether the UE supports Type 1 PUSCH transmissions with configured grant as specified in TS 38.214 [12] with UL-TWG-repK value of one. This applies only to non-shared spectrum channel access. For shared spectrum channel access, *configuredUL-GrantType1-r16* applies. UE shall set the capability value consistently for all FDD-FR1 bands, all TDD-FR1 bands, all TDD-FR2-1 bands and all TDD-FR2-2 bands respectively.The UE only includes *configuredUL-GrantType1-v1650* if *configuredUL-GrantType1* is absent. | Band | No | N/A | N/A |
| ***configuredUL-GrantType2-v1650***Indicates whether the UE supports Type 2 PUSCH transmissions with configured grant as specified in TS 38.214 [12] with UL-TWG-repK value of one. This applies only to non-shared spectrum channel access. For shared spectrum channel access, *configuredUL-GrantType2-r16* applies. UE shall set the capability value consistently for all FDD-FR1 bands, all TDD-FR1 bands, all TDD-FR2-1 bands and all TDD-FR2-2 bands respectively.The UE only includes *configuredUL-GrantType2*-v1650 if *configuredUL-GrantType2* is absent. | Band | No | N/A | N/A |
| ***cqi-4-BitsSubbandNTN-SharedSpectrumChAccess-r17***Indicates whether the UE supports CQI reporting with 4 bits per subband for NTN and shared spectrum channel access. | Band | No | N/A | N/A |
| ***crossCarrierScheduling-SameSCS***Indicates whether the UE supports cross carrier scheduling for the same numerology with carrier indicator field (CIF) in carrier aggregation where numerologies for the scheduling cell and scheduled cell are same. | Band | No | N/A | N/A |
| ***csi-ReportFramework***Indicates whether the UE supports CSI report framework. This capability signalling comprises the following parameters:- *maxNumberPeriodicCSI-PerBWP-ForCSI-Report* indicates the maximum number of periodic CSI report setting per BWP for CSI report;- *maxNumberPeriodicCSI-PerBWP-ForBeamReport* indicates the maximum number of periodic CSI report setting per BWP for beam report.- *maxNumberAperiodicCSI-PerBWP-ForCSI-Report* indicates the maximum number of aperiodic CSI report setting per BWP for CSI report;- *maxNumberAperiodicCSI-PerBWP-ForBeamReport* indicates the maximum number of aperiodic CSI report setting per BWP for beam report;- *maxNumberAperiodicCSI-triggeringStatePerCC* indicates the maximum number of aperiodic CSI triggering states in *CSI-AperiodicTriggerStateList* per CC;- *maxNumberSemiPersistentCSI-PerBWP-ForCSI-Report* indicates the maximum number of semi-persistent CSI report setting per BWP for CSI report;- *maxNumberSemiPersistentCSI-PerBWP-ForBeamReport* indicates the maximum number of semi-persistent CSI report setting per BWP for beam report;- *simultaneousCSI-ReportsPerCC* indicates the number of CSI report(s) for which the UE can measure and process reference signals simultaneously in a CC of the band for which this capability is provided. The CSI report comprises periodic, semi-persistent and aperiodic CSI and any latency classes and codebook types. The CSI report in simultaneousCSI-ReportsPerCC includes the beam report and CSI report.The UE is mandated to report *csi-ReportFramework*. | Band | Yes | N/A | N/A |
| ***csi-ReportFrameworkExt-r16***Indicates whether the UE supports the extension of the maximum number of configured aperiodic CSI report settings for all codebook types. The capability signalling comprises the following:*maxNumberAperiodicCSI-PerBWP-ForCSI-ReportExt-r16* indicates the extended maximum number of aperiodic CSI report setting per BWP for CSI report. If present, the value of *maxNumberAperiodicCSI-PerBWP-ForCSI-Report-r16* shall replace the corresponding value in *csi-ReportFramework*. | Band | No | N/A | N/A |
| ***csi-RS-ForTracking***Indicates support of CSI-RS for tracking (i.e. TRS). This capability signalling comprises the following parameters:- *maxBurstLength* indicates the TRS burst length. Value 1 indicates 1 slot and value 2 indicates both of 1 slot and 2 slots. In this release UE is mandated to report value 2;- *maxSimultaneousResourceSetsPerCC* indicates the maximum number of TRS resource sets per CC which the UE can track simultaneously;- *maxConfiguredResourceSetsPerCC* indicates the maximum number of TRS resource sets configured to UE per CC. It is mandated to report at least 8 for FR1 and 16 for FR2;- *maxConfiguredResourceSetsAllCC* indicates the maximum number of TRS resource sets configured to UE across CCs. If the UE includes the field in an FR1 band, it shall set the same value in all FR1 bands. If the UE includes the field in an FR2 band, it shall set the same value in all FR2 bands. The UE supports a total number of resources equal to the maximum of the FR1 and FR2 value, but no more than the FR1 value across all FR1 serving cells and no more than the FR2 value across all FR2 serving cells. The UE is mandated to report at least 16 for FR1 and 32 for FR2.The UE is mandated to report *csi-RS-ForTracking*. | Band | Yes | N/A | N/A |
| ***csi-RS-IM-ReceptionForFeedback***Indicates support of CSI-RS and CSI-IM reception for CSI feedback. This capability signalling comprises the following parameters:- *maxConfigNumberNZP-CSI-RS-PerCC* indicates the maximum number of configured NZP-CSI-RS resources per CC;- *maxConfigNumberPortsAcrossNZP-CSI-RS-PerCC* indicates the maximum number of ports across all configured NZP-CSI-RS resources per CC;- *maxConfigNumberCSI-IM-PerCC* indicates the maximum number of configured CSI-IM resources per CC;- *maxNumberSimultaneousNZP-CSI-RS-PerCC* indicates the maximum number of simultaneous CSI-RS-resources per CC;- *totalNumberPortsSimultaneousNZP-CSI-RS-PerCC* indicates the total number of CSI-RS ports in simultaneous CSI-RS resources per CC.The UE is mandated to report csi-RS-IM-ReceptionForFeedback. | Band | Yes | N/A | N/A |
| ***csi-RS-ProcFrameworkForSRS***Indicates support of CSI-RS processing framework for SRS. This capability signalling comprises the following parameters:- *maxNumberPeriodicSRS-AssocCSI-RS-PerBWP* indicates the maximum number of periodic SRS resources associated with CSI-RS per BWP;- *maxNumberAperiodicSRS-AssocCSI-RS-PerBWP* indicates the maximum number of aperiodic SRS resources associated with CSI-RS per BWP;- *maxNumberSP-SRS-AssocCSI-RS-PerBWP* indicates the maximum number of semi-persistent SRS resources associated with CSI-RS per BWP;- *simultaneousSRS-AssocCSI-RS-PerCC* indicates the number of SRS resources that the UE can process simultaneously in a CC, including periodic, aperiodic and semi-persistent SRS. | Band | No | N/A | N/A |
| ***defaultQCL-PerCORESETPoolIndex-r16***Indicates whether the UE supports default QCL assumption per CORESET pool index using multi-DCI based multi-TRP. The UE that indicates support of this feature shall support *multiDCI-MultiTRP-r16* and *simultaneousReceptionDiffTypeD-r16.* | Band | No | N/A | FR2 only |
| ***defaultQCL-TwoTCI-r16***Indicates whether the UE supports default QCL assumption with two TCI states using single-DCI based multi-TRP. The UE can include this field only if *simultaneousReceptionDiffTypeD-r16*is present. Otherwise, the UE does not include this field. | Band | No | N/A | FR2 only |
| ***dmrs-BundlingNonBackToBackTX-r17***Indicates whether the UE supports DM-RS bundling for non-back-to-back transmission for consecutive slots for PUSCH and PUCCH only for corresponding supported back-to-back transmission as reported in *dmrs-BundlingPUSCH-RepTypeA-r17*, *dmrs-BundlingPUSCH-RepTypeB-r17*, *dmrs-BundlingPUSCH-multiSlot-r17* or *dmrs-BundlingPUCCH-Rep-r17*. The UE is considered to support the feature in a band of a band combination if the UE indicates support of the feature for the corresponding band and for the band combination[, except for the case where the band combination consists only of a band with a single component carrier, the feature is supported based on the UE indicating support of the feature for the corresponding band].UE indicating support of this feature shall also indicate support of at least one of dmrs-BundlingPUSCH-RepTypeA-r17, dmrs-BundlingPUSCH-RepTypeB-r17, dmrs-BundlingPUSCH-multiSlot-r17 or dmrs-BundlingPUCCH-Rep-r17. | Band | No | N/A | N/A |
| ***dmrs-BundlingPUCCH-Rep-r17***Indicates whether the UE supports DM-RS bundling for PUCCH repetitions for PUCCH formats 1/3/4 over consecutive symbols. The UE is considered to support the feature in a band of a band combination if the UE indicates support of the feature for the corresponding band and for the band combination[, except for the case where the band combination consists only of a band with a single component carrier, the feature is supported based on the UE indicating support of the feature for the corresponding band].UE indicating support of this feature shall also indicate support of *maxDurationDMRS-Bundling-r17* and *pucch-Repetition-F1-3-4*. | Band | No | N/A | N/A |
| ***dmrs-BundlingPUSCH-multiSlot-r17***Indicates whether the UE supports DM-RS bundling for TB processing over multi-slot PUSCH over consecutive symbols. The UE is considered to support the feature in a band of a band combination if the UE indicates support of the feature for the corresponding band and for the band combination[, except for the case where the band combination consists only of a band with a single component carrier, the feature is supported based on the UE indicating support of the feature for the corresponding band].UE indicating support of this feature shall also indicate support of *maxDurationDMRS-Bundling-r17* and *tb-ProcessingMultiSlotPUSCH-r17*. | Band | No | N/A | N/A |
| ***dmrs-BundlingPUSCH-RepTypeA-r17***Indicates whether the UE supports DM-RS bundling for PUSCH repetition type A over consecutive symbols. The UE is considered to support the feature in a band of a band combination if the UE indicates support of the feature for the corresponding band and for the band combination[, except for the case where the band combination consists only of a band with a single component carrier, the feature is supported based on the UE indicating support of the feature for the corresponding band].UE indicating support of this feature shall also indicate support of *maxDurationDMRS-Bundling-r17* and at least one of *type1-PUSCH-RepetitionMultiSlots*, *type2-PUSCH-RepetitionMultiSlots* or *pusch-RepetitionMultiSlots*. | Band | No | N/A | N/A |
| ***dmrs-BundlingPUSCH-RepTypeB-r17***Indicates whether the UE supports DM-RS bundling for PUSCH repetition type B over consecutive symbols. The UE is considered to support the feature in a band of a band combination if the UE indicates support of the feature for the corresponding band and for the band combination[, except for the case where the band combination consists only of a band with a single component carrier, the feature is supported based on the UE indicating support of the feature for the corresponding band].UE indicating support of this feature shall also indicate support of *maxDurationDMRS-Bundling-r17* and *pusch-RepetitionTypeB-r16*. | Band | No | N/A | N/A |
| ***dmrs-BundlingRestart-r17***Indicates whether the UE supports restarting DM-RS bundling after the events triggered by DCI or MAC CE that violate power consistency and phase continuity. The UE is considered to support the feature in a band of a band combination if the UE indicates support of the feature for the corresponding band and for the band combination[, except for the case where the band combination consists only of a band with a single component carrier, the feature is supported based on the UE indicating support of the feature for the corresponding band].UE indicating support of this feature shall also indicate support of *maxDurationDMRS-Bundling-r17.*NOTE: Events which are triggered by DCI or MAC CE, but do not require UE capability to resume maintaining power consistency and/or phase continuity as specified in clause 6.1.7 of TS 38.214 [12] are excluded from this feature. | Band | No | N/A | N/A |
| ***dynamicMulticastDCI-Format4-2-r17***Indicates whether the UE supports DCI format 4\_2 with CRC scrambled with G-RNTI for multicast.A UE supporting this feature shall also indicate support of *dynamicMulticastPCell-r17*. | Band | No | N/A | N/A |
| ***dynamicSlotRepetitionMulticastNTN-SharedSpectrumChAccess-r17***Indicates the maximum number of supported dynamic slot-level repetitions for group-common PDSCH for multicast for NTN and shared spectrum channel access. Value n8 corresponds to 8, and value n16 corresponds to 16.A UE supporting this feature shall also indicate support of *dynamicMulticastPCell-r17*. | Band | No | N/A | N/A |
| ***dynamicSlotRepetitionMulticastTN-NonSharedSpectrumChAccess-r17***Indicates the maximum number of supported dynamic slot-level repetitions for group-common PDSCH for multicast for TN and non-shared spectrum channel access. Value n8 corresponds to 8, and value n16 corresponds to 16. UE shall set the capability value consistently for all FDD-FR1 bands, all TDD-FR1 bands, all TDD-FR2 bands respectively.A UE supporting this feature shall also indicate support of *dynamicMulticastPCell-r17*. | Band | No | N/A | N/A |
| ***enhancedSkipUplinkTxConfigured-v1660***Indicates whether the UE supports skipping UL transmission for a configured uplink grant only if no data is available for transmission and no UCI is multiplexed on the corresponding PUSCH of the uplink grant as specified in TS 38.321 [8]. UE shall set the capability value consistently for all FDD-FR1 bands, all TDD-FR1 bands, all TDD-FR2-1 bands and all TDD-FR2-2 bands respectively.The UE only includes *enhancedSkipUplinkTxConfigured-v1660* if *enhancedSkipUplinkTxConfigured-r16* is absent. | Band | No | N/A | N/A |
| ***enhancedSkipUplinkTxDynamic-v1660***Indicates whether the UE supports skipping UL transmission for an uplink grant addressed to a C-RNTI only if no data is available for transmission and no UCI is multiplexed on the corresponding PUSCH of the uplink grant as specified in TS 38.321 [8]. UE shall set the capability value consistently for all FDD-FR1 bands, all TDD-FR1 bands, all TDD-FR2-1 bands and all TDD-FR2-2 bands respectively.The UE only includes *enhancedSkipUplinkTxDynamic-v1660* if *enhancedSkipUplinkTxDynamic-r16* is absent. | Band | No | N/A | N/A |
| ***enhancedType3-HARQ-CodebookFeedback-r17***Indicates whether the UE supports enhanced type 3 HARQ-ACK codebook feedback based on triggering information in DCI 1\_1 and DCI 1\_2 (for a UE supporting DCI format 1\_2 as indicated in *dci-Format1-2And0-2-r16*) and also supports transmission of enhanced type 3 HARQ-ACK codebook using the first or second PUCCH configuration based on PHY priority indication in the triggering DCI (for a UE supporting two HARQ-ACK codebooks / PUCCH config as indicated in twoHARQ-ACK-Codebook-type1-r16). The capability signalling comprises the following parameters:- *enhancedType3-HARQ-Codebooks-r17* indicates the maximum number of supported enhanced type 3 HARQ-ACK codebooks;- *maxNumberPUCCH-Transmissions-r17* indicates the maximum number of actual PUCCH transmissions for type 3 or enhanced type 3 HARQ-ACK codebook feedback within a slot.UE only supports feedback of a dynamically selected enhanced type 3 HARQ-ACK codebook based on triggering information in DCI 1\_1 and DCI 1\_2 (for a UE supporting DCI format 1\_2 as indicated in *dci-Format1-2And0-2-r16*) if the UE supports more than one enhanced type 3 HARQ-ACK codebook to be configured (as indicated in *enhancedType3-HARQ-Codebooks-r17*). The UE indicates support of this capability shall also indicates support of *oneShotHARQ-feedback-r16*. | Band | No | N/A | N/A |
| ***enhancedUL-TransientPeriod-r16***Indicates whether the UE supports enhanced UL performance for the transient period as specified in clause 6.3.3 of TS 38.101-1 [2]. If not reported, the UE supports transient period of 10us. | Band | No | N/A | FR1 only |
| ***eventA4BasedCondHandover-r17***Indicates whether the UE supports Event A4 based conditional handover, i.e., *CondEvent A4* as specified in TS 38.331 [9]. A UE supporting this feature shall also indicate the support of *condHandover-r16* for NTN bands and the support of *nonTerrestrialNetwork-r17*. UE shall set the capability value consistently for all FDD-FR1 NTN bands. | Band | No | N/A | N/A |
| ***extendedCP***Indicates whether the UE supports 60 kHz subcarrier spacing with extended CP length for reception of PDCCH, and PDSCH, and transmission of PUCCH, PUSCH, and SRS. | Band | No | N/A | N/A |
| ***groupBeamReporting***Indicates whether UE supports RSRP reporting for the group of two reference signals. | Band | No | N/A | N/A |
| ***groupSINR-reporting-r16***Indicates whether UE supports group based L1-SINR reporting. UE indicates support of this feature shall indicate support of *ssb-csirs-SINR-measurement-r16.* | Band | No | N/A | N/A |
| ***handoverUTRA-FDD-r16***Indicates whether the UE supports NR to UTRA-FDD CELL\_DCH CS handover for the PCell on the band. It is mandatory to support both UTRA-FDD measurement and event B triggered reporting, and periodic UTRA-FDD measurement and reporting if the UE supports HO to UTRA-FDD. If this field is included, then UE shall support IMS voice over NR. UE shall set the capability value consistently for all FDD-FR1 bands, all TDD-FR1 bands, all TDD-FR2-1 bands and all TDD-FR2-2 bands respectively. | Band | No | N/A | N/A |
| ***interSlotFreqHopInterSlotBundlingPUSCH-r17***Indicates whether the UE supports enhanced inter-slot frequency hopping with inter-slot bundling for PUSCH.UE indicating support of this feature shall also indicate support of at least one of *dmrs-BundlingPUSCH-RepTypeA-r17*, *dmrs-BundlingPUSCH-RepTypeB-r17* or *dmrs-BundlingPUSCH-multiSlot-r17*. | Band | No | N/A | N/A |
| ***interSlotFreqHopPUCCH-r17***Indicates whether the UE supports enhanced inter-slot frequency hopping for PUCCH repetitions with DMRS bundling.UE indicating support of this feature shall also indicate support of *dmrs-BundlingPUCCH-Rep-r17*. | Band | No | N/A | N/A |
| ***maxDurationDMRS-Bundling-r17***Indicates whether the UE supports the maximum duration during which UE is able to maintain power consistency and phase continuity to support DM-RS bundling for PUSCH/PUCCH.NOTE: DM-RS bundling is only applicable for UL transmissions with pi/2 BPSK, BPSK, and QPSK modulation orders for the corresponding physical channels. | Band | No | N/A | N/A |
| ***maxMIMO-LayersForMulti-DCI-mTRP-r16***Indicates the interpretation of *maxNumberMIMO-LayersPDSCH* for multi-DCI based mTRP. If this field is included, *maxNumberMIMO-LayersPDSCH* is interpreted as the maximum number of layers per PDSCH for multi-DCI multi-TRP operation.If this field is not included, *maxNumberMIMO-LayersPDSCH* is interpreted as the maximum number of layers across two PDSCHs if having at least one RE overlapped, for multi-DCI multi-TRP operation. The UE that indicates support of this feature shall support *overlapPDSCHsFullyFreqTime-r16*.NOTE 1: For data rate calculation in clause 4.1.2, if this feature is indicated, each multi-DCI based multi-TRP CC is counted two times toward J. | Band | No | N/A | N/A |
| ***max-HARQ-ProcessNumber-r17***Indicates the maximal supported HARQ process numbers for UL and for DL respectively. For each value of *max-HARQ-ProcessNumber-r17*, value *u16d32* indicates the maximal supported HARQ process number is 16 for UL and 32 for DL, value *u32d16* indicates the maximal supported HARQ process number is 32 for UL and 16 for DL, value *u32d32* indicates the maximal supported HARQ process number is 32 for UL and 32 for DL. This field is only applicable for bands in Table 5.2.2-1 in TS 38.101-5 [34] and HAPS operation bands in clause 5.2 of TS 38.104 [35]. | Band | No | N/A | N/A |
| ***maxNumberPUSCH-TypeA-Repetition-r17***Indicates whether the UE supports the increased maximum number of PUSCH Type A repetitions to 32.A UE that indicates support of this feature shall support *type1-PUSCH-RepetitionMultiSlots, type2-PUSCH-RepetitionMultiSlots* or *pusch-RepetitionTypeA-r16.*NOTE: For DG PUSCH, the number of repetitions is indicated in a TDRA list. A row index of the TDRA list is indicated by a DCI. For Type 1 CG PUSCH, the number of repetitions is indicated by *repK-v1710*. For Type 2 CG PUSCH, the number of repetitions is indicated in a TDRA list or by *repK-v1710*. | Band | No | N/A | N/A |
| ***mux-HARQ-ACK-DiffPriorities-r17***Indicates whether the UE supports HARQ-ACK with different priorities multiplexing on a PUCCH/PUSCH, comprised of the following functional components:- Supports multiplexing a high-priority HARQ-ACK and a low-priority HARQ-ACK into a PUCCH. Supports separate coding for the two HARQ-ACKs;- Supports multiplexing a low-priority HARQ-ACK, a high-priority HARQ-ACK and a high-priority SR into a PUCCH;- Supports multiplexing a low-priority HARQ-ACK in a high-priority PUSCH (conveying UL-SCH only). Supports separate beta\_offset values for this priority combination;- Supports multiplexing a high-priority HARQ-ACK in a low-priority PUSCH (conveying UL-SCH only). Supports separate beta\_offset values for this priority combination;- Supports multiplexing a low-priority HARQ-ACK, a high-priority PUSCH, a high-priority HARQ-ACK and/or CSI;- Supports multiplexing a high-priority HARQ-ACK, a low-priority PUSCH, a low-priority HARQ-ACK and/or CSI.The UE indicating support of this feature shall also indicate the support of *twoHARQ-ACK-Codebook-type1-r16.* | Band | No | N/A | N/A |
| ***jointReleaseConfiguredGrantType2-r16***Indicates whether the UE supports joint release in a DCI for two or more configured grant Type 2 configurations for a given BWP of a serving cell. The UE can include this feature only if the UE indicates support of *activeConfiguredGrant-r16*. | Band | No | N/A | N/A |
| ***jointReleaseSPS-r16***Indicates whether the UE supports joint release in a DCI for two or more SPS configurations for a given BWP of a serving cell. The UE can include this feature only if the UE indicates support of *sps-r16*. | Band | No | N/A | N/A |
| ***k1-RangeExtension-r17***Indicates whether the UE supports extended K1 value range of (0..31) for unpaired spectrum. This field is only applicable for bands in Table 5.2.2-1 in TS 38.101-5 [34] and HAPS operation bands in clause 5.2 of TS 38.104 [35]. | Band | No | N/A | N/A |
| ***locationBasedCondHandover-r17***Indicates whether the UE supports location based conditional handover, i.e., *CondEvent D1* as specified in TS 38.331 [9]. A UE supporting this feature shall also indicate the support of *condHandover-r16* for NTN bands and the support of *nonTerrestrialNetwork-r17*. UE shall set the capability value consistently for all FDD-FR1 NTN bands. | Band | No | N/A | N/A |
| ***lowPAPR-DMRS-PDSCH-r16***Indicates whether the UE supports low PAPR DMRS for PDSCH. | Band | No | N/A | N/A |
| ***lowPAPR-DMRS-PUCCH-r16***Indicates whether the UE supports low PAPR DMRS for PUCCH format 3 and format 4 with transform precoding and with pi/2 BPSK modulation. UE indicates support of this feature shall indicate support of *pucch-F3-4-HalfPi-BPSK* and any combination of support of *pucch-F3-WithFH*, *pucch-F4-WithFH* and *pucch-F1-3-4WithoutFH*. It is mandatory with capability signalling. | Band | Yes | N/A | N/A |
| ***lowPAPR-DMRS-PUSCHwithoutPrecoding-r16***Indicates whether the UE supports low PAPR DMRS for PUSCH without transform precoding. | Band | No | N/A | N/A |
| ***lowPAPR-DMRS-PUSCHwithPrecoding-r16***Indicates whether the UE supports low PAPR DMRS for PUSCH with transform precoding and with pi/2 BPSK modulation. It is mandatory with capability signalling. UE indicates support of this feature shall indicate support of *pusch-HalfPi-BPSK*. | Band | Yes | N/A | N/A |
| ***maxModulationOrderForMulticast-r17***Defines the maximal modulation order for multicast PDSCH. If not reported, UE supports the same modulation order as unicast.- For FR1, up to 1024QAM is supported.- For FR2, up to 256QAM is supported.A UE supporting this feature shall also indicate support of *dynamicMulticastPCell-r17*.NOTE: A UE shall support the corresponding mandatory maximum modulation for unicast. | Band | No | N/A | N/A |
| ***maxNumberActivatedTCI-States-r16***Indicates maximum number of activated TCI states. This capability signalling includes the following:- *maxNumberPerCORESET-Pool-r16* indicates maximal number of activated TCI states per *CORESETPoolIndex* per BWP per CC including data and control- *maxTotalNumberAcrossCORESET-Pool-r16* indicates maximal total number of activated TCI states across *CORESETPoolIndex* per BWP per CC including data and controlThe UE that indicates support of this feature shall support *multiDCI-MultiTRP-r16*. | Band | No | N/A | N/A |
| ***maxNumberCSI-RS-BFD***Indicates maximal number of CSI-RS resources across all CCs, and across MCG and SCG in case of NR-DC, for UE to monitor PDCCH quality. In this release, the maximum value that can be signalled is 16. If the UE includes the field in an FR1 band, it shall set the same value in all FR1 bands. If the UE includes the field in an FR2 band, it shall set the same value in all FR2 bands. The UE supports a total number of resources equal to the maximum of the FR1 and FR2 value, but no more than the FR1 value across all FR1 serving cells and no more than the FR2 value across all FR2 serving cells. It is mandatory with capability signalling for FR2 and optional for FR1. | Band | CY | N/A | N/A |
| ***maxNumberCSI-RS-SSB-CBD***Defines maximal number of different CSI-RS [and/or SSB] resources across all CCs, and across MCG and SCG in case of NR-DC, for new beam identifications. In this release, the maximum value that can be signalled is 128. If the UE includes the field in an FR1 band, it shall set the same value in all FR1 bands. If the UE includes the field in an FR2 band, it shall set the same value in all FR2 bands. The UE supports a total number of resources equal to the maximum of the FR1 and FR2 value, but no more than the FR1 value across all FR1 serving cells and no more than the FR2 value across all FR2 serving cells. It is mandatory with capability signalling for FR2 and optional for FR1. The UE is mandated to report at least 32 for FR2. | Band | CY | N/A | N/A |
| ***maxNumberG-CS-RNTI-r17***Defines maximum number of G-CS-RNTIs for SPS multicast. For TN, the UE shall set the capability value consistently for all FDD-FR1 bands, all TDD-FR1 bands and all TDD-FR2 bands, associated with supported shared and non-shared spectrum respectively. For NTN, UE shall set the capability value consistently for all FDD-FR1 NTN bands.A UE supporting this feature shall also indicate support of *sps-Multicast-r17*. | Band | No | N/A | N/A |
| ***maxNumberG-RNTI-r17***Defines maximum number of G-RNTIs for multicast. For TN, the UE shall set the capability value consistently for all FDD-FR1 bands, all TDD-FR1 bands and all TDD-FR2 bands, associated with supported shared and non-shared spectrum respectively. For NTN, UE shall set the capability value consistently for all FDD-FR1 NTN bands.A UE supporting this feature shall also indicate support of *dynamicMulticastPCell-r17*. | Band | No | N/A | N/A |
| ***maxNumberNonGroupBeamReporting***Defines support of non-group based RSRP reporting using N\_max RSRP values reported. | Band | Yes | N/A | N/A |
| ***maxNumberRxBeam, maxNumberRxBeam-v1720***Defines whether UE supports receive beamforming switching using NZP CSI-RS resource. UE shall indicate a single value for the preferred number of NZP CSI-RS resource repetitions per CSI-RS resource set. Support of Rx beam switching is mandatory for FR2. | Band | CY | N/A | N/A |
| ***maxNumberRxTxBeamSwitchDL,*** ***maxNumberRxTxBeamSwitchDL-v1710***Defines the number of Tx and Rx beam changes UE can perform on this band within a slot. UE shall report one value per each subcarrier spacing supported by the UE. In this release, the number of Tx and Rx beam changes for scs-15kHz and scs-30kHz are not included. | Band | No | N/A | FR2 only |
| ***maxNumberSCellBFR-r16***Defines the maximum number of SCells configured for SCell beam failure recovery simultaneously. The UE indicating support of this also indicates the capabilities of *maxNumberCSI-RS-BFD, maxNumberSSB-BFD* and *maxNumberCSI-RS-SSB-CBD.* | Band | No | N/A | N/A |
| ***maxNumberSSB-BFD***Defines maximal number of different SSBs across all CCs, and across MCG and SCG in case of NR-DC, for UE to monitor PDCCH quality. In this release, the maximum value that can be signalled is 16. If the UE includes the field in an FR1 band, it shall set the same value in all FR1 bands. If the UE includes the field in an FR2 band, it shall set the same value in all FR2 bands. The UE supports a total number of resources equal to the maximum of the FR1 and FR2 value, but no more than the FR1 value across all FR1 serving cells and no more than the FR2 value across all FR2 serving cells. It is mandatory with capability signalling for FR2 and optional for FR1. | Band | CY | N/A | N/A |
| ***maxNumber-LEO-SatellitesPerCarrier-r17***Indicates the number of target LEO satellites the UE can monitor per carrier. For serving carrier, the number of target LEO satellites also includes the serving satellite. If this field is not included, the number of target satellites UE can monitor per carrier is 2. The value shall be larger than or equal to the reported value on *maxNumber-NGSO-SatellitesWithinOneSMTC-r17*. | Band | No | FDD only | FR1 only |
| ***maxNumber-NGSO-SatellitesWithinOneSMTC-r17***Indicates the number of different NGSO satellites for target cells that the UE supports of simultaneous measurements within a SMTC with value n1 corresponds to 1, value n2 corresponds to 2 and so on. | Band | No | FDD only | FR1 only |
| ***maxUplinkDutyCycle-PC2-FR1***Indicates the maximum percentage of symbols during a certain evaluation period that can be scheduled for uplink transmission so as to ensure compliance with applicable electromagnetic energy absorption requirements provided by regulatory bodies. This field is only applicable for FR1 power class 2 UE as specified in clause 6.2.1 of TS 38.101-1 [2]. If the field is absent, 50% shall be applied. Value n60 corresponds to 60%, value n70 corresponds to 70% and so on. This capability is not applicable to IAB-MT. | Band | No | N/A | FR1 only |
| ***maxUplinkDutyCycle-FR2***Indicates the maximum percentage of symbols during 1s that can be scheduled for uplink transmission at the UE maximum transmission power, so as to ensure compliance with applicable electromagnetic power density exposure requirements provided by regulatory bodies. This field is applicable for all power classes UE in FR2 as specified in TS 38.101-2 [3]. Value n15 corresponds to 15%, value n20 corresponds to 20% and so on. If the field is absent or the percentage of uplink symbols transmitted within any 1s evaluation period is larger than *maxUplinkDutyCycle-FR2*, the UE behaviour is specified in TS 38.101-2 [3]. This capability is not applicable to IAB-MT. | Band | No | N/A | FR2 only |
| ***maxUplinkDutyCycle-PC1dot5-MPE-FR1-r16***Indicates the maximum percentage of symbols during a certain evaluation period that can be scheduled for uplink transmission so as to ensure compliance with applicable electromagnetic energy absorption requirements provided by regulatory bodies. This field is only applicable for FR1 power class 1.5 UE as specified in clause 6.2.1 of TS 38.101-1 [2]. If the field is absent, UE shall mitigate MPE autonomously by P-MPR or by other means and no restriction on scheduled uplink duty cycle is needed. | Band | No | N/A | FR1 only |
| ***mn-InitiatedCondPSCellChangeNRDC-r17***Indicates whether the UE supports MN initiated conditional PSCell change in NR-DC, which is configured by NR *conditionalReconfiguration* using MN configured measurement as triggering condition. The UE supporting this feature shall also support 2 trigger events for same execution condition in MN initiated conditional PSCell change in NR-DC. UE shall set the capability value consistently for all FDD-FR1 bands, all TDD-FR1 bands and all TDD-FR2 bands respectively. | Band | No | N/A | N/A |
| ***modifiedMPR-Behaviour***Indicates whether UE supports modified MPR behaviour defined in TS 38.101-1 [2] and TS 38.101-2 [3]. | Band | No | N/A | N/A |
| ***mpr-PowerBoost-FR2-r16***Indicates whether UE supports uplink transmission power boost by suspension of in-band emission (IBE) requirements as specified in TS 38.101-2 [3]. | Band | No | TDD only | FR2 only |
| ***mpe-Mitigation-r17***Indicates the support of enhanced PHR reporting which includes pairs of (P-MPR, SSBRI/CRI).This feature also includes following parameters:- *maxNumP-MPR-RI-pairs-r17* indicates the maximum number of reported P-MPR and SSBRI/CRI pairs;- *maxNumConfRS-r17* indicates the maximum number of candidate RS(s) configured in a RRC pool for MPE mitigation.NOTE: *maxNumConfRS-r17* is also counted in *maxTotalResourcesForOneFreqRange-r16*/ *maxTotalResourcesForAcrossFreqRanges-r16.* | Band | No | N/A | FR2 only |
| ***mTRP-PUCCH-InterSlot-r17***Indicates whether the UE supports the following features:- support of PUCCH repetition scheme 1 (inter-slot repetition) with sequential mapping for repetitions larger than 2 and with cyclic mapping for 2 repetitions.- support of up to two PUCCH power control parameter sets/spatial relation information per PUCCH resource. The power control parameter sets only apply to FR1 and spatial relation information only applies to FR2.- supported PUCCH formats for PUCCH repetition scheme 1. | Band | No | N/A | N/A |
| ***mTRP-PUCCH-CyclicMapping-r17***Indicates whether the UE supports cyclic mapping for beam mapping/power control parameter set mapping for PUCCH repetitions scheme 1 and/or 3 when the number of repetitions is larger than 2.The UE that indicates support of this feature shall also indicate support of *mTRP-PUCCH-InterSlot-r17.* | Band | No | N/A | N/A |
| ***mTRP-PUCCH-SecondTPC-r17***Indicates whether the UE supports second TPC field for per TRP closed-loop power control for PUCCH with DCI formats 1\_1 / 1\_2.The UE that indicates support of this feature shall also indicate support of *mTRP-PUCCH-InterSlot-r17.* | Band | No | N/A | N/A |
| ***mTRP-PUSCH-twoCSI-RS-r17***Indicates whether the UE supports up to two NZP CSI-RS resources associated with the two SRS resource sets for non-codebook-based mTRP PUSCH.The UE that indicates support of this feature shall also indicate support of *srs-AssocCSI-RS, csi-RS-IM-ReceptionForFeedbackPerBandComb and mTRP-PUSCH-RepetitionTypeA-r17.* | Band | No | N/A | N/A |
| ***mTRP-BFR-twoBFD-RS-Set-r17***Indicates whether the UE supports mTRP BFR based on two BFD-RS sets. The capability signalling comprises the following parameters:*-* *maxBFD-RS-resourcesPerSetPerBWP-r17* indicates the maximum number of supported measured BFD-RS resources per set per BWP.- *maxBFR-r17* indicates the maximum number of CCs per band configured with BFR (including spCell/SCell/MTRP BFR).*-* *maxBFD-RS-resourcesAcrossSetsPerBWP-r17* indicates the supported maximum number of measured BFD-RS resources across two BFD-RS sets per BWP.*maxBFD-RS-resourcesAcrossSetsPerBWP-r17* is also counted in *maxTotalResourcesForOneFreqRange-r16* and *maxTotalResourcesForAcrossFreqRanges-r16*. | Band | No | N/A | N/A |
| ***mTRP-BFR-PUCCH-SR-perCG-r17***Indicates the maximum number of supported PUCCH-SR resources for MTRP BFR per cell group. A UE that supports *mTRP-BFR-twoBFD-RS-Set-r17* shall indicate support of this feature with at least 1 PUCCH-SR resources for MTRP BFR per cell group.UE shall set the capability value consistently for all FDD-FR1 bands, all TDD-FR1 bands, all TDD-FR2-1 bands and all TDD-FR2-2 bands respectively. | Band | No | N/A | N/A |
| ***mTRP-BFR-association-PUCCH-SR-r17***Indicates whether the UE supports association between a BFD-RS resource set on SpCell and a PUCCH SR resource.The UE indicating support of this feature shall support *mTRP-BFR-PUCCH-SR-perCG-r17.* UE shall set the capability value consistently for all FDD-FR1 bands, all TDD-FR1 bands, all TDD-FR2-1 bands and all TDD-FR2-2 bands respectively. | Band | No | N/A | N/A |
| ***mTRP-BFD-RS-MAC-CE-r17***Indicates the support of MAC-CE based update of explicit BFD-RS for mTRP BFR with maximum number of configured candidate BFD-RS per BWP for MAC-CE based update.The UE indicating support of this feature shall also indicate the support of *mTRP-BFR-twoBFD-RS-Set-r17*. | Band | No | N/A | N/A |
| ***mTRP-CSI-EnhancementPerBand-r17***Indicates support of CSI enhancements for multi-TRP including support of NZP CSI-RS resource pairs used as CMR (channel measurement resource) pairs for NCJT measurement hypothesis with N=1.This feature also includes following parameters:- *maxNumNZP-CSI-RS-r17* indicates the maximum number of NZP CSI-RS resources in one CSI-RS resource set: Ks,max- *cSI-Report-mode-r17* indicates the CSI report mode selection. Mode1 indicates mode 1 with X=0, mode2 indicates mode 2, both indicate the support of both mode 1 with X=0 and mode 2.- A list of supported combinations, up to 16, across all CCs simultaneously, where each combination includes:- *maxNumTx-Ports-r17* indicates the maximum number of Tx ports in one NZP CSI-RS resource associated with an NCJT measurement hypothesis- *maxTotalNumCMR-r17* indicates the maximum total number of CMRs for NCJT measurement- *maxTotalNumTx-PortsNZP-CSI-RS-r17* indicates the maximum total number of Tx ports of NZP CSI-RS resources associated with NCJT measurement hypotheses- *codebookModeNCJT-r17* indicates the supported codebook modes for NCJT CSI. | Band | No | N/A | N/A |
| ***mTRP-CSI-numCPU-r17***Indicates the number of CSI processing units (CPUs) occupied by a pair of CMRs for NCJT CSI hypotheses. Maximum number of CPUs is reported in *csi-ReportFramework*.The UE indicating support of this feature shall also indicate the support of *mTRP-CSI-EnhancementPerBand-r17*. | Band | No | N/A | N/A |
| ***mTRP-CSI-additionalCSI-r17***Indicates the maximum value of *numberOfSingleTRP-CSI-Mode1*.The UE indicating support of this feature shall also indicate 'mode1' or 'both' in *cSI-Report-mode-r17* of *mTRP-CSI-EnhancementPerBand-r17*. | Band | No | N/A | N/A |
| ***mTRP-CSI-N-Max2-r17***Indicates the support of maximum number of CMR pairs Nmax=2 configured in *NZP-CSI-RS-ResourceSet* for a given CSI report setting.The UE indicating support of this feature shall also indicate the support of *mTRP-CSI-EnhancementPerBand-r17.* | Band | No | N/A | N/A |
| ***mTRP-CSI-CMR-r17***Indicates the support of a NZP CSI-RS resource referred by both a CMR pair configured for Rel-17 Multi-TRP CSI enhancement and a single CMR configured for Single-TRP measurement in a CSI reporting setting.The UE indicating support of this feature shall also indicate the support of *mTRP-CSI-EnhancementPerBand-r17*. | Band | No | N/A | FR2 only |
| ***mTRP-PDCCH-individual-r17***Indicates the support of monitoring of individual candidates when one of the linked PDCCH candidates uses the same set of CCEs as an individual (unlinked) PDCCH candidate, and they both are associated with the same DCI size, scrambling, and CORESET.The UE indicating support of this feature shall also indicate support of *mTRP-PDCCH-Repetition-r17*. | Band | No | N/A | N/A |
| ***mTRP-PDCCH-anySpan-3Symbols-r17***Indicates support of PDCCH repetition for PDCCH monitoring on any span of up to 3 consecutive OFDM symbols of a slot. It is applicable to 15kHz SCS only.The UE indicating support of this feature shall also indicate support of *pdcchMonitoringSingleOccasion* and *mTRP-PDCCH-Repetition-r17*. | Band | No | N/A | FR1 only |
| ***mTRP-PDCCH-TwoQCL-TypeD-r17*** Indicates the support of determining two QCL-TypeD for time-domain overlapping CORESETs in the same CC or for intra-band CA when UE is configured with PDCCH repetition.The UE indicating support of this feature shall also indicate support of *mTRP-PDCCH-Repetition-r1*7. | Band | No | N/A | FR2 only |
| ***mTRP-PUSCH-CSI-RS-r17***Indicates the support of CSI-RS processing framework for SRS with two associated CSI-RS resources.This feature also includes following parameters:- *maxNumPeriodicSRS-r17* indicates the maximum number of periodic SRS resources associated with first and second CSI-RS per BWP.- *maxNumAperiodicSRS-r17* indicates the maximum number of aperiodic SRS resources associated with first and second CSI-RS per BWP.- *maxNumSP-SRS-r17* indicates the maximum number of semi-persistent SRS resources associated with first and second CSI-RS per BWP.- *numSRS-ResourcePerCC-r17*: UE can process Y SRS resources associated with first and second CSI-RS resources simultaneously in a CC. Includes Periodic/Semi-Persistent/Aperiodic SRS.- *numSRS-ResourceNonCodebook-r17*: UE can process up to X CSI-RS resources associated with SRS for non-codebook based transmission simultaneously.The UE indicating support of this feature shall also indicate the support of *mTRP-PUSCH-twoCSI-RS-r17.* | Band | No | N/A | N/A |
| ***mTRP-PUSCH-cyclicMapping-r17***Indicates the support of cyclic mapping when the number of repetitions is larger than 2 with repetition type.The UE indicating support of this feature shall also indicate the support of *mTRP-PUSCH-TypeA-CB-r17*or *mTRP-PUSCH-RepetitionTypeA-r17*. | Band | No | N/A | N/A |
| ***mTRP-PUSCH-secondTPC-r17***Indicates the support of second TPC field for per TRP closed-loop power control for PUSCH with DCI formats 0\_1 and 0\_2.The UE indicating support of this feature shall also indicate the support of *mTRP-PUSCH-TypeA-CB-r17*or *mTRP-PUSCH-RepetitionTypeA-r17.* | Band | No | N/A | N/A |
| ***mTRP-PUSCH-twoPHR-Reporting-r17***Indicates the support of PHR reporting related to M-TRP PUSCH repetition (calculate two PHRs (at least corresponding to the CC that applies m-TRP PUSCH repetitions), each associated with a first PUSCH occasion corresponding to each SRS resource set, and report two PHRs).The UE indicating support of this feature shall also indicate the support of *mTRP-PUSCH-TypeA-CB-r17* or *mTRP-PUSCH-RepetitionTypeA-r17.* | Band | No | N/A | N/A |
| ***mTRP-PUSCH-A-CSI-r17***Indicates the support of A-CSI report on two PUSCH repetitions.The UE indicating support of this feature shall also indicate the support of *mTRP-PUSCH-TypeA-CB-r17*or *mTRP-PUSCH-RepetitionTypeA-r17.* | Band | No | N/A | N/A |
| ***mTRP-PUSCH-SP-CSI-r17***Indicates the support of SP-CSI report on two PUSCH repetitions.The UE indicating support of this feature shall also indicate the support of *mTRP-PUSCH-TypeA-CB-r17*or *mTRP-PUSCH-RepetitionTypeA-r17.* | Band | No | N/A | N/A |
| ***mTRP-PUSCH-CG-r17***Indicates the support of CG PUSCH transmission towards M-TRPs using a single CG configuration. The UE uses same beam mapping principals as dynamic grant PUSCH repetition scheme.The UE indicating support of this feature shall also indicate the support of *mTRP-PUSCH-TypeA-CB-r17*or *mTRP-PUSCH-RepetitionTypeA-r17*. | Band | No | N/A | N/A |
| ***mTRP-PUCCH-MAC-CE-r17***Indicates the support of updating two Spatial Relation Info's and two sets of power control parameters for a group of PUCCH resources in a CC by MAC-CE.The UE indicates support of this feature shall also indicate support of *mTRP-PUCCH-InterSlot-r17.* | Band | No | N/A | N/A |
| ***mTRP-PUCCH-maxNum-PC-FR1-r17***Indicates the maximum number of power control parameter sets configured for multi-TRP PUCCH repetition in FR1.The UE indicating support of this feature shall also indicate the support of *mTRP-PUCCH-InterSlot-r17.* | Band | No | N/A | FR1 only |
| ***mTRP-inter-Cell-r17***Indicates the support of RRC configuration of additional PCI different from serving cell associated with the TCI state and/or QCL-info.This feature also includes following parameters:- *maxNumAdditionalPCI-Case1-r17* indicates the maximum number of configured additional PCIs per CC is X1 (Case 1) when each configuration of SSB time domain positions and periodicity of the additional PCIs is the same as SSB time domain positions and periodicity of the serving cell PCI.- *maxNumAdditionalPCI-Case2-r17* indicates the maximum number of configured additional PCIs per CC is X2 (Case 2) when the configurations of SSB time domain positions and periodicity of the additional PCIs is not according to Case 1.The UE indicating support of this feature shall also indicate the support of *multiDCI-MultiTRP-r16.* | Band | No | N/A | N/A |
| ***mTRP-GroupBasedL1-RSRP-r17***Indicates the support of group based L1-RSRP reporting enhancements.This feature also includes following parameters:- *maxNumBeamGroups-r17* indicates the maximum number N of beam groups (M=2 beams per beam group) in a single L1-RSRP reporting instance based on measurement on two CMR resource sets.- *maxNumRS-WithinSlot-r17* indicates the maximum number of SSB and CSI-RS resources for measurement in both CMR sets within a slot across all CCs.*-* *maxNumRS-AcrossSlot-r17* indicates the maximum number of configured SSB and CSI-RS resources for measurement in both CMR sets across all CCs.*maxNumRS-WithinSlot-r17* and *maxNumRS-AcrossSlot-r17* are also counted in *maxTotalResourcesForOneFreqRange-r16* and *maxTotalResourcesForAcrossFreqRanges-r16*. | Band | No | N/A | N/A |
| ***multiPDSCH-SingleDCI-FR2-1-SCS-120kHz-r17***Indicates whether the UE supports multi-PDSCH scheduling by single DCI for the operation with 120kHz SCS in FR2-1 and HARQ enhancements for both type 1 and type 2 HARQ codebook. | Band | No | N/A | N/A |
| ***multiPUSCH-SingleDCI-FR2-1-SCS-120kHz-r17***Indicates whether the UE supports multi-PUSCH scheduling by single DCI for the operation with 120kHz SCS in FR2-1 with non-contiguous allocation. | Band | No | N/A | N/A |
| ***multipleRateMatchingEUTRA-CRS-r16***Indicates whether the UE supports multiple E-UTRA CRS rate matching patterns, which is supported only for FR1. The capability signalling comprises the following parameters:- *maxNumberPatterns-r16* indicates the maximum number of LTE-CRS rate matching patterns in total within a NR carrier using 15 kHz SCS. The UE can report the value larger than 2 only if UE reports the value of *maxNumberNon-OverlapPatterns-r16* is larger than 1.- *maxNumberNon-OverlapPatterns-r16* indicates the maximum number of LTE-CRS non-overlapping rate matching patterns within a NR carrier using 15 kHz SCS.The UE can include this feature only if the UE indicates support of *rateMatchingLTE-CRS*. | Band | No | N/A | FR1 only |
| ***multipleTCI***Indicates whether UE supports more than one TCI state configurations per CORESET. UE is only required to track one active TCI state per CORESET. UE is required to support minimum between 64 and number of configured TCI states indicated by *tci-StatePDSCH*. This field shall be set to *supported*. | Band | Yes | N/A | N/A |
| ***nack-OnlyFeedbackForMulticastWithDCI-Enabler-r17***Indicates whether the UE supports DCI-based enabling/disabling NACK-only based HARQ-ACK feedback configured per G-RNTI by RRC signalling via DCI format 4\_2.A UE supporting this feature shall also indicate support of *nack-OnlyFeedbackForMulticast-r17* and *dynamicMulticastDCI-Format4-2-r17*. | Band | No | N/A | N/A |
| ***nonGroupSINR-reporting-r16***Indicates N\_max L1-SINR values reported when UE supports non-group based L1-SINR reporting. UE indicates support of this feature shall indicate support of *ssb-csirs-SINR-measurement-r16.* | Band | No | N/A | N/A |
| ***nr-UE-TxTEG-ID-MaxSupport-r17***Indicates the maximum number of UE TxTEG for SRS resource for positioning, which is supported and reported by UE for UL TDOA. The UE can include this field only if the UE supports *srs-AllPosResources-r16*. | Band | No | N/A | N/A |
| ***olpc-SRS-Pos-r16***Indicates whether the UE supports OLPC for SRS for positioning. The capability signalling comprises the following parameters.- *olpc-SRS-PosBasedOnPRS-Serving-r16* indicates whether the UE supports OLPC for SRS for positioning based on PRS from the serving cell in the same band. The UE can include this field only if the UE supports *NR-DL-PRS-ProcessingCapability-r16* defined in TS 37.355 [22], and *srs-PosResources-r16*. Otherwise, the UE does not include this field;- *olpc-SRS-PosBasedOnSSB-Neigh-r16* indicates whether the UE supports OLPC for SRS for positioning based on SSB from the neighbouring cell in the same band. The UE can include this field only if the UE supports *srs-PosResources-r16*. Otherwise, the UE does not include this field;- *olpc-SRS-PosBasedOnPRS-Neigh-r16* indicates whether the UE supports OLPC for SRS for positioning based on PRS from the neighbouring cell in the same band. The UE can include this field only if the UE supports *olpc-SRS-PosBasedOnPRS-Serving-r16*. Otherwise, the UE does not include this field;NOTE: A PRS from a PRS-only TP is treated as PRS from a non-serving cell.- *maxNumberPathLossEstimatePerServing-r16* indicates the maximum number of pathloss estimates that the UE can simultaneously maintain for all the SRS resource sets for positioning per serving cell in addition to the up to four pathloss estimates that the UE maintains per serving cell for the PUSCH/PUCCH/SRS transmissios. The UE shall include this field if the UE supports any of *olpc-SRS-PosBasedOnPRS-Serving-r16, olpc-SRS-PosBasedOnSSB-Neigh-r16* and *olpc-SRS-PosBasedOnPRS-Neigh-r16.* Otherwise, the UE does not include this field. | Band | No | N/A | N/A |
| ***olpc-SRS-PosRRC-Inactive-r17***Indicates whether the UE supports OLPC for SRS for positioning in RRC\_INACTIVE. The capability signalling comprises the following parameters.- *olpc-SRS-PosBasedOnPRS-Serving-r16* indicates whether the UE supports OLPC for SRS for positioning based on PRS from the serving cell in the same band. The UE can include this field only if the UE supports *NR-DL-PRS-ProcessingCapability-r16* defined in TS 37.355 [22], and *srs-PosResourcesRRC-Inactive-r17*. Otherwise, the UE does not include this field;- *olpc-SRS-PosBasedOnSSB-Neigh-r16* indicates whether the UE supports OLPC for SRS for positioning based on SSB from the neighbouring cell in the same band. The UE can include this field only if the UE supports *srs-PosResourcesRRC-Inactive-r17*. Otherwise, the UE does not include this field;- *olpc-SRS-PosBasedOnPRS-Neigh-r16* indicates whether the UE supports OLPC for SRS for positioning based on PRS from the neighbouring cell in the same band. The UE can include this field only if the UE supports *olpc-SRS-PosBasedOnPRS-Serving-r16*. Otherwise, the UE does not include this field;NOTE: A PRS from a PRS-only TP is treated as PRS from a non-serving cell.*-* *maxNumberPathLossEstimatePerServing-r16* indicates the maximum number of pathloss estimates that the UE can simultaneously maintain for all the SRS resource sets for positioning per serving cell in addition to the up to four pathloss estimates that the UE maintains per serving cell for the PUSCH/PUCCH/SRS transmissions. The UE shall include this field if the UE supports any of *olpc-SRS-PosBasedOnPRS-Serving-r16, olpc-SRS-PosBasedOnSSB-Neigh-r16* and *olpc-SRS-PosBasedOnPRS-Neigh-r16.* Otherwise, the UE does not include this field. | Band | No | N/A | N/A |
| ***oneShotHARQ-feedbackPhy-Priority-r17***Indicates whether the UE supports transmission of type 3 HARQ-ACK codebook using the first or second PUCCH configuration based on PHY priority indication in the triggering DCI.A UE supporting this feature shall also indicate support of *oneShotHARQ-feedback-r16* and *twoHARQ-ACK-Codebook-type1-r16*. | Band | No | N/A | N/A |
| ***oneShotHARQ-feedbackTriggeredByDCI-1-2-r17***Indicates whether the UE supports one-shot HARQ ACK feedback triggered by DCI format 1\_2, comprised of the following functional components:-Supports feedback of type 3 HARQ-ACK codebook, triggered by a DCI 1\_2 scheduling a PDSCH;-Supports feedback of type 3 HARQ-ACK codebook, triggered by a DCI 1\_2 without scheduling a PDSCH using a reserved FDRA value.A UE supporting this feature shall also indicate support of *oneShotHARQ-feedback-r16* and *dci-Format1-2And0-2-r16*. | Band | No | N/A | N/A |
| ***oneSlotPeriodicTRS-r16***Indicates whether the UE supports one-slot periodic TRS configuration only when no two consecutive slots are indicated as downlink slots by *tdd-UL-DL-ConfigurationCommon* or *tdd-UL-DL-ConfigDedicated*. If the UE supports this feature, the UE needs to report *csi-RS-ForTracking*. | Band | No | TDD only | FR1 only |
| ***outOfOrderOperationDL-r16***Indicates whether the UE supports out of order operation for DL. The UE that indicates support of this feature shall support *multiDCI-MultiTRP-r16*. The capability signalling comprises the following parameters:*- supportPDCCH-ToPDSCH-r16* indicates support out-of-order operation for PDCCH to PDSCH;*- supportPDSCH-ToHARQ-ACK-r16* indicates support out-of-order operation for PDSCH to HARQ-ACK. | Band | No | N/A | N/A |
| ***outOfOrderOperationUL-r16***Indicates whether the UE supports out of order operation for UL. The UE that indicates support of this feature shall support *multiDCI-MultiTRP-r16.*Note: Same closed loop index for power control across PUSCHs associated with different *CORESETPoolIndex* values is not supported by a UE indicating the support of this feature when TPC accumulation is enabled. | Band | No | N/A | N/A |
| ***overlapPDSCHsFullyFreqTime-r16***Indicates the maximal number of PDSCH scrambling sequences per serving cell when the UE supports PDSCHs with fully overlapping Resource Elements. The UE that indicates support of this feature shall support *multiDCI-MultiTRP-r16.*Note: A UE may assume that its maximum receive timing difference between the DL transmissions from two TRPs is within a Cyclic Prefix | Band | No | N/A | N/A |
| ***overlapPDSCHsInTimePartiallyFreq-r16***Indicates whether the UE supports PDSCHs with partially overlapping Resource Elements. The UE that indicates support of this feature shall support *overlapPDSCHsFullyFreqTime-r16.* | Band | No | N/A | N/A |
| ***overlapRateMatchingEUTRA-CRS-r16***Indicates whether the UE supports two LTE-CRS overlapping rate matching patterns within a part of NR carrier using 15 kHz SCS overlapping with a LTE carrier. If the UE supports this feature, the UE needs to report *multipleRateMatchingEUTRA-CRS-r16*. | Band | No | N/A | FR1 only |
| ***parallelMeasurementWithoutRestriction-r17***Indicates whether the UE supports measurements on cells belonging to different satellites as the serving cell in parallel with normal operation (i.e. data/control transmission and/or reception, and L1 measurements) of serving cell without scheduling restrictions. The feature is applicable only when the serving satellite is NGSO. If the serving cell belongs to GSO satellite, the scheduling restriction is not applied on the premise that a mixed type of satellites on the same frequency layer is not supported in this release. If not reported, for measurements in parallel with normal operation of serving cell scheduling restrictions shall apply. | Band | No | FDD only | FR1 only |
| ***parallelPRS-MeasRRC-Inactive-r17***Indicates whether the UE supports performing RRM measurement and PRS measurement in parallel. UE shall set the capability value consistently for all FDD-FR1 bands, all TDD-FR1 bands, all TDD-FR2-1 bands and all TDD-FR2-2 bands respectively | Band | No | N/A | N/A |
| ***pdcch-SkippingWithoutSSSG-r17***Indicates whether the UE supports up to 2-bit indication of PDCCH skipping by scheduling DCI if SSSG is not configured as specified in TS 38.213 [11], clause 10.4. | Band | No | N/A | N/A |
| ***pdcch-SkippingWithSSSG-r17***Indicates whether the UE supports 2-bit indication of SSSG switching between 2 SSSGs, PDCCH skipping by scheduling DCI, and timer based SSSG switching as specified in TS 38.213 [11], clause 10.4. UE supports search space set group switching capability-1 according to Table 10.4-1 of TS 38.213 [11].UE indicating support of this feature shall also indicate support of *pdcch-SkippingWithoutSSSG-r17* and *sssg-Switching-1bitInd-r17*. | Band | No | N/A | N/A |
| ***pdsch-1024QAM-2MIMO-FR1-r17***Indicates whether the UE supports 1024QAM modulation scheme for PDSCH with maximum 2 MIMO layers for FR1 as defined in TS 38.211 [6], MCS and CQI feedback tables based on 1024QAM modulation order as defined in TS 38.214 [12].UE indicating support of this feature shall also indicate support of *pdsch-256QAM-FR1* and shall not indicate support of *pdsch-1024QAM-FR1-r17*. | Band | No | N/A | FR1 only |
| ***pdsch-1024QAM-FR1-r17***Indicates whether the UE supports 1024QAM modulation scheme for PDSCH for FR1 as defined in TS 38.211 [6], MCS and CQI feedback tables based on 1024QAM modulation order as defined in TS 38.214 [12].UE indicating support of this feature shall also indicate support of *pdsch-256QAM-FR1* and shall not indicate support of *pdsch-1024QAM-2MIMO-FR1-r17*. | Band | No | N/A | FR1 only |
| ***pdsch-256QAM-FR2***Indicates whether the UE supports 256QAM modulation scheme for PDSCH for FR2 as defined in 7.3.1.2 of TS 38.211 [6]. | Band | No | N/A | FR2 only |
| ***pdsch-MappingTypeB-Alt-r16***Indicates whether the UE supports PDSCH Type B scheduling of length 9 and 10 OFDM symbols, and DMRS shift for length-10 symbols. If the UE supports this feature, the UE needs to report *pdsch-MappingTypeB*. | Band | No | N/A | FR1 only |
| ***periodicBeamReport***Indicates whether UE supports periodic 'CRI/RSRP' or 'SSBRI/RSRP' reporting using PUCCH formats 2, 3 and 4 in one slot. | Band | Yes | N/A | N/A |
| ***posSRS-RRC-Inactive-OutsideInitialUL-BWP-r17***Indicates support of Positioning SRS transmission in RRC\_INACTIVE state configured outside initial UL BWP. The capability signalling comprises the following parameters:- *maxSRSposBandwidthForEachSCS-withinCC-FR1-r17* Indicates the maximum SRS bandwidth supported for each SCS that UE supports within a single CC for FR1*;*- *maxSRSposBandwidthForEachSCS-withinCC-FR2-r17* indicates the maximum SRS bandwidth supported for each SCS that UE supports within a single CC for FR2;- *maxNumOfSRSposResourceSets-r17* indicates the max number of SRS Resource Sets for positioning supported by UE;- *maxNumOfPeriodicSRSposResources-r17* indicates the max number of periodic SRS Resources for positioning;- *maxNumOfPeriodicSRSposResourcesPerSlot-r17* indicates the max number of periodic SRS Resources for positioning per slot;- *differentNumerologyBetweenSRSposAndInitialBWP-r17* indicates the support of different numerology between the SRS and the initial UL BWP;- *srsPosWithoutRestrictionOnBWP-r17* indicates the support of SRS operation without restriction on the BW: BW of the SRS may not include BW of the CORESET#0 and SSB;- *maxNumOfPeriodicAndSemipersistentSRSposResources-r17* indicates the max number of P/SP SRS Resources for positioning;- *maxNumOfPeriodicAndSemipersistentSRSposResourcesPerSlot-r17* indicates the max number of P/SP SRS Resources for positioning per slot;- *differentCenterFreqBetweenSRSposAndInitialBWP-r17* indicates the support of a different center frequency between the SRS for positioning and the initial UL BWP;- *switchingTimeSRS-TX-OtherTX-r17* indicates the switching time between SRS TX and other TX in initial UL BWP or RX in initial DL BWP- *maxNumOfSemiPersistentSRSposResources-r17* indicates the max number of semi-persistent SRS Resources for positioning;- *maxNumOfSemiPersistentSRSposResourcesPerSlot-r17* indicates the max number of semi-persistent SRS Resources for positioning per slot.The UE can include this field only if the UE supports *srs-PosResourcesRRC-Inactive-r17*. Otherwise, the UE does not include this field;NOTE 1: The SRS should have a *locationAndBandwidth*, SCS, CP, defined the same way as a legacy BWP.NOTE 2: If *differentCenterFreqBetweenSRSposAndInitialBWP-r17* is not signalled, the UE only supports same center frequency between the SRS for positioning and initial UL BWP.NOTE 3: If *differentNumerologyBetweenSRSposAndInitialBWP-r17* is not signalled, the UE only supports same numerology between the SRS and the initial UL BWP.NOTE 4: If *srsPosWithoutRestrictionOnBWP-r17* is not signalled, the UE supports only SRS BW that include the BW of the CORESET #0 and SSB.NOTE 5: The fields of *maxNumOfSemiPersistentSRSposResources-r17* and *maxNumOfSemiPersistentSRSposResourcesPerSlot-r17* shall be reported together if supported by UE. One of the fields between *maxSRSposBandwidthForEachSCS-withinCC-FR1-r17* and *maxSRSposBandwidthForEachSCS-withinCC-FR2-r17,* and the fields of *maxNumOfSRSposResourceSets-r17, maxNumOfPeriodicSRSposResources-r17, maxNumOfPeriodicSRSposResourcesPerSlot-r17, maxNumOfPeriodicAndSemipersistentSRSposResources-r17, maxNumOfPeriodicAndSemipersistentSRSposResourcesPerSlot-r17,* and *switchingTimeSRS-TX-OtherTX-r17* shall be reported together if supported by UE.NOTE 6: *srsPosWithoutRestrictionOnBWP-r17* is not applicable to FDD or SUL bands. | Band | No | N/A | N/A |
| ***powerBoosting-pi2BPSK***Indicates whether UE supports power boosting for pi/2 BPSK, when applicable as defined in 6.2 of TS 38.101-1 [2] v16.9.0. It is mandatory with capability signalling. This capability is not applicable to IAB-MT. | Band | CY | TDD only | FR1 only |
| ***prs-MeasurementWithoutMG-r17***Indicates whether the UE supports using the threshold to compare the Rx time difference between the serving cell and a neighbor cell/TRP for PRS measurements, as defined in clause 9.9.1.2 of TS 38.133 [5], to determine whether the PRS from the non-serving cell satisfy the condition of PRS measurement outside MG. The UE can include this field only if the UE supports one of *prs-ProcessingWindowType1A-r17, prs-ProcessingWindowType1B-r17* and *prs-ProcessingWindowType2-r17*. | Band | No | N/A | N/A |
| ***prs-ProcessingCapabilityOutsideMGinPPW-r17***Indicates the DL-PRS Processing Capability outside MG and comprises the following subfields:- *prsProcessingType-r17****:*** Indicates the DL-PRS Processing Window Type for which the *prs-ProcessingCapabilityOutsideMGinPPW-r17* are provided.- *ppw-dl-PRS-BufferType-r17*: Indicates DL-PRS buffering capability. Value *'type1'* indicates sub-slot/symbol level buffering and value *'type2'* indicates slot level buffering.- *ppw-durationOfPRS-Processing1-r17*: Indicates the duration of DL-PRS symbols N in units of ms a UE can process every T ms assuming maximum DL-PRS bandwidth provided in *ppw-maxNumOfDL-Bandwidth-r17* and comprises the following subfields- *ppw-durationOfPRS-ProcessingSymbolsN-r17*: This field specifies the values for *N* with values msDot125 indicates 0.125ms, msDot25 indicates 0.25ms, and so on- *ppw-durationOfPRS-ProcessingSymbolsT-r17*: This field specifies the values for *T* with values ms1 indicates 1ms, ms2 indicates 2ms, and so on.- *ppw-durationOfPRS-Processing2-r17*: Indicates the duration of DL-PRS symbols N2 in units of ms a UE can process every T2 ms assuming maximum DL-PRS bandwidth provided in *ppw-maxNumOfDL-Bandwidth-r17* and comprises the following subfields:- *ppw-durationOfPRS-ProcessingSymbolsN2-r17*: This field specifies the values for *N2* with values msDot125 indicates 0.125ms, msDot25 indicates 0.25ms, and so on.- *ppw-durationOfPRS-ProcessingSymbolsT2-r17*: This field specifies the values for *T2* with values ms4 indicates 4ms, ms5 indicates 5ms, and so on.- *ppw-maxNumOfDL-PRS-ResProcessedPerSlot-r17*: Indicates the maximum number of DL PRS bandwidth in MHz, which is supported and reported by UE for PRS measurement outside MG within the PPW.- *ppw-maxNumOfDL-Bandwidth-r17*: Indicates the maximum number of DL PRS bandwidth in MHz for FR1 and FR2, which is supported and reported by UE for PRS measurement outside MG within the PPW.The UE can include this field only if the UE supports one of *prs-ProcessingWindowType1A-r17*, *prs-ProcessingWindowType1B-r17* and *prs-ProcessingWindowType2-r17*. Otherwise, the UE does not include this field.NOTE: A UE that supports one of *prs-ProcessingWindowType1A-r17*, *prs-ProcessingWindowType1B-r17* or *prs-ProcessingWindowType2-r17* shall always support *ppw-dl-PRS-BufferType-r17*, *ppw-durationOfPRS-Processing1-r17*, *ppw-durationOfPRS-Processing2-r17*, *ppw-maxNumOfDL-PRS-ResProcessedPerSlot-r17*, and *ppw-maxNumOfDL-Bandwidth-r17*. | Band | No | N/A | N/A |
| ***prs-ProcessingRRC-Inactive-r17***Indicates whether the UE supports PRS processing in RRC\_INACTIVE. | Band | No | N/A | N/A |
| ***prs-ProcessingWindowType1A-r17***Indicates whether the UE supports PRS processing Type 1A, subject to the UE determining that DL PRS to be higher priority for PRS measurement outside MG and in a PRS processing window and the priority handling options of PRS as follows:- Option 1: Support of "st1" and "st3" defined in clause 5.1.6.5 of TS 38.214 [12].- Option 2: Support of "st1", "st2", and "st3" defined in clause 5.1.6.5 of TS 38.214 [12].NOTE 1: Void.- Option 3: Support of "st1" only defined in clause 5.1.6.5 of TS 38.214 [12].The UE can include this field only if the UE supports *prs-ProcessingCapabilityBandList-r16* defined in TS 37.355 [22].A UE supporting this feature shall also indicate support of *prs-ProcessingCapabilityOutsideMGinPPW-r17*.NOTE 2: Type 1A refers to the determination of prioritization between DL PRS and other DL signals/channels in all OFDM symbols within the PRS processing window. The DL signals/channels from all DL CCs (per UE) are affected across LTE and NR.NOTE 3: Within a PRS processing window, UE measurement is inside the active DL BWP with PRS having the same numerology as the active DL BWP.NOTE 4: Support of configuration of PRS processing window in RRC and support of using DL MAC CE to activate/deactivate the PRS processing window for PRS measurements is part of the feature. | Band | No | N/A | N/A |
| ***prs-ProcessingWindowType1B-r17***Indicates whether the UE supports PRS processing Type 1B, subject to the UE determining that DL PRS to be higher priority for PRS measurement outside MG and in a PRS processing window and the priority handling options of PRS as follows:- Option 1: Support of "st1" and "st3" defined in clause 5.1.6.5 of TS 38.214 [12].- Option 2: Support of "st1", "st2", and "st3" defined in clause 5.1.6.5 of TS 38.214 [12].NOTE 1: Void.- Option 3: Support of "st1" only defined in clause 5.1.6.5 of TS 38.214 [12].The UE can include this field only if the UE supports *prs-ProcessingCapabilityBandList-r16* defined in TS 37.355 [22].A UE supporting this feature shall also indicate support of *prs-ProcessingCapabilityOutsideMGinPPW-r17*.NOTE 2: Type 1B refers to the determination of prioritization between DL PRS and other DL signals/channels in all OFDM symbols within the PRS processing window. The DL signals/channels from a certain band are affected.NOTE 3: Within a PRS processing window, UE measurement is inside the active DL BWP with PRS having the same numerology as the active DL BWP.NOTE 4: Support of configuration of PRS processing window in RRC and support of using DL MAC CE to activate/deactivate the PRS processing window for PRS measurements is part of the feature. | Band | No | N/A | N/A |
| ***prs-ProcessingWindowType2-r17***Indicates whether the UE supports PRS processing Type 2, subject to the UE determining that DL PRS to be higher priority for PRS measurement outside MG and in a PRS processing window and the priority handling options of PRS as follows:- Option 1: Support of "st1" and "st3" defined in clause 5.1.6.5 of TS 38.214 [12].- Option 2: Support of "st1", "st2", and "st3" defined in clause 5.1.6.5 of TS 38.214 [12].NOTE 1: Void.- Option 3: Support of "st1" only defined in clause 5.1.6.5 of TS 38.214 [12].The UE can include this field only if the UE supports *prs-ProcessingCapabilityBandList-r16* defined in TS 37.355 [22].A UE supporting this feature shall also indicate support of *prs-ProcessingCapabilityOutsideMGinPPW-r17*.NOTE 2: Type 2 refers to the determination of prioritization between DL PRS and other DL signals/channels only in DL PRS symbols within the PRS processing window.NOTE 3: Within a PRS processing window, UE measurement is inside the active DL BWP with PRS having the same numerology as the active DL BWP.NOTE 4: Support of configuration of PRS processing window in RRC and support of using DL MAC CE to activate/deactivate the PRS processing window for PRS measurements is part of the feature. | Band | No | N/A | N/A |
| ***ptrs-DensityRecommendationSetDL***For each supported sub-carrier spacing, indicates preferred threshold sets for determining DL PTRS density. It is mandated for FR2. For each supported sub-carrier spacing, this field comprises:- two values of *frequencyDensity*;- three values of *timeDensity*. | Band | CY | N/A | N/A |
| ***ptrs-DensityRecommendationSetUL***For each supported sub-carrier spacing, indicates preferred threshold sets for determining UL PTRS density. For each supported sub-carrier spacing, this field comprises:- two values of *frequencyDensity*;- three values of *timeDensity*;- five values of *sampleDensity*. | Band | No | N/A | N/A |
| ***pucch-Repetition-F0-2-r17***Indicates whether the UE supports transmission of a PUCCH format 0 and 2 over multiple slots with the repetition factor 2, 4 or 8.A UE supporting this feature shall also indicate support of *pucch-Repetition-F1-3-4*. | Band | No | N/A | N/A |
| ***pucch-SpatialRelInfoMAC-CE***Indicates whether the UE supports indication of *PUCCH-spatialrelationinfo* by a MAC CE per PUCCH resource. It is mandatory for FR2 and optional for FR1. | Band | CY | N/A | N/A |
| ***pusch-256QAM***Indicates whether the UE supports 256QAM modulation scheme for PUSCH as defined in 6.3.1.2 of TS 38.211 [6]. | Band | No | N/A | N/A |
| ***pusch-RepetitionMsg3-r17***Indicates whether the UE supports repetition of PUSCH transmission scheduled by RAR UL grant and DCI format 0\_0 with CRC scrambled by TC-RNTI. | Band | No | N/A | N/A |
| ***pusch-RepetitionMultiSlots-v1650***Indicates whether the UE supports transmitting PUSCH scheduled by DCI format 0\_1 when configured with higher layer parameter *pusch-AggregationFactor* > 1, as defined in clause 6.1.2.1 of TS 38.214 [12]. This applies only to non-shared spectrum channel access. For shared spectrum channel access, *pusch-RepetitionMultiSlots-r16* applies. UE shall set the capability value consistently for all FDD-FR1 bands, all TDD-FR1 bands, all TDD-FR2-1 bands and all TDD-FR2-2 bands respectively.The UE only includes *pusch-RepetitionMultiSlots-v1650* if *pusch-RepetitionMultiSlots* is absent. | Band | Yes | N/A | N/A |
| ***pusch-TransCoherence***Defines support of the uplink codebook subset by the UE for UL precoding for PUSCH transmission as described in clause 6.1.1.1 of TS 38.214 [12]. UE indicated support of partial coherent codebook subset shall also support non-coherent codebook subset. UE indicated support of full coherent codebook subset shall also support partial and non-coherent codebook subset. | Band | No | N/A | N/A |
| ***puschTypeA-RepetitionsAvailSlot-r17***Indicates whether UE supports dynamic and configured grant PUSCH repetitions based on available slots. Transmission occasions for the repetitions for dynamic and configured grant PUSCH are determined on the basis of available slots.A UE that indicates support of this feature shall support *type1-PUSCH-RepetitionMultiSlots, type2-PUSCH-RepetitionMultiSlots* or *pusch-RepetitionMultiSlots.* | Band | No | N/A | N/A |
| ***rateMatchingLTE-CRS***Indicates whether the UE supports receiving PDSCH with resource mapping that excludes the REs determined by the higher layer configuration LTE-carrier configuring common RS, as specified in TS 38.214 [12]. | Band | Yes | N/A | N/A |
| ***re-LevelRateMatchingForMulticast-r17***Indicates whether the UE supports group-common PDSCH RE-level rate matching for multicast, comprised of the following functional components:- Supports SP ZP-CSI-RS for group-common PDSCH RE-mapping patterns;- Supports P ZP-CSI-RS for group-common PDSCH RE-mapping patterns;- Supports *p-ZP-CSI-RS-ResourceSet* configured in *PDSCH-Config-Multicast* same as or different from the *p-ZP-CSI-RS-ResourceSet* configured in *PDSCH-Config*;- Supports AP ZP-CSI-RS for group-common PDSCH RE-mapping patterns.For TN, the UE shall set the capability value consistently for all FDD-FR1 bands, all TDD-FR1 bands and all TDD-FR2 bands, associated with supported shared and non-shared spectrum respectively. For NTN, UE shall set the capability value consistently for all FDD-FR1 NTN bands.A UE supporting this feature shall also indicate support of *dynamicMulticastPCell-r17*. A UE supporting this feature in FR1 bands shall also indicate support of *pdsch-RE-MappingFR1-PerSymbol* or *pdsch-RE-MappingFR1-PerSlot*. A UE supporting this feature in FR2 bands shall also indicate support of *pdsch-RE-MappingFR2-PerSymbol* or *pdsch-RE-MappingFR2-PerSlot*.NOTE: The total number of semi-persistent ZP-CSI-RS-ResourceSet that a UE can be configured with is the same as for unicast in Rel-16. | Band | No | N/A | N/A |
| ***rlm-Relaxation-r17***Indicates whether the UE supports RLM relaxation criteria and requirement as specified in TS 38.133 [5]. UE shall set the capability value consistently for all FDD-FR1 bands, all TDD-FR1 bands, all TDD-FR2-1 bands and all TDD-FR2-2 bands respectively.UE indicating support of this feature shall also indicate support of *ssb-RLM* and/or *csi-RS-RLM.* | Band | No | N/A | N/A |
| ***searchSpaceSetGrp-switchCap2-r17***Indicates whether UE supports search space set group switching capability 2 for FR1 according to Table 10.4-1 of TS 38.213 [11] for SSSG switching.UE indicating support of this feature shall also indicate support of *sssg-Switching-1bitInd-r17*.NOTE: For UE supporting this feature and also *sssg-Switching-1BitInd-r17*, *sssg-Switching-2BitInd-r17*, and/or *pdcch-SkippingWithSSSG-r17*, search space set group switching Capability-2 is applied to *sssg-Switching-1BitInd-r17*, *sssg-Switching-2BitInd-r17*, and/or *pdcch-SkippingWithSSSG-r17*. | Band | No | N/A | FR1 only |
| ***semi-PersistentL1-SINR-Report-PUCCH-r16***Indicates whether the UE supports semi-persistent L1-SINR report on PUCCH. The UE indicating support of this feature shall include at least one of the following capabilities:- *supportReportFormat1-2OFDM-syms-r16* indicates support of report on PUCCH formats over 1 – 2 OFDM symbols once per slot (or piggybacked on a PUSCH)- *supportReportFormat4-14OFDM-syms-r16* indicates support of report on PUCCH formats over 4 – 14 OFDM symbols once per slot (or piggybacked on a PUSCH).The UE indicating support of this feature shall also indicate support of *ssb-csirs-SINR-measurement-r16.*  | Band | No | N/A | N/A |
| ***semi-PersistentL1-SINR-Report-PUSCH-r16***Indicates whether the UE supports semi-persistent L1-SINR report on PUSCH. The UE indicating support of this feature shall also indicate support of *ssb-csirs-SINR-measurement-r16.*  | Band | No | N/A | N/A |
| ***separateCRS-RateMatching-r16***Indicates whether the UE supports rate match around configured CRS patterns which is associated with *CORESETPoolIndex* (if configured) and are applied to the PDSCH scheduled with a DCI detected on a CORESET with the same value of *CORESETPoolIndex*. The UE that indicates support of this feature shall support *multiDCI-MultiTRP-r16* and *overlapRateMatchingEUTRA-CRS-r16.* This is only applicable for 15kHz SCS. | Band | No | N/A | FR1 only |
| ***sfn-SimulTwoTCI-AcrossMultiCC-r17***Indicates whether the UE supports simultaneous activation of two TCI states for CORESETs with the same CORESET ID in all BWPs across a set of configured component carriers by single MAC-CE. The UE indicating support of this feature shall also indicate *sfn-schemeA-r17* or *sfn-schemeB-r17* or *sfn-SchemeA-PDCCH-only-r17*.The UE shall set the capability value consistently for all FDD-FR1 bands, all TDD-FR1 bands, all TDD-FR2-1 bands and all TDD-FR2-2 bands respectively. | Band | No | N/A | N/A |
| ***sfn-DefaultDL-BeamSetup-r17***Indicates whether the UE supports the following features:- For FR2 only, PDSCH reception using default beam for enhanced SFN scheme when PDSCH is scheduled with offset less than threshold.- For FR1 and FR2, PDSCH reception using default beam for enhanced SFN scheme when TCI field is not present in DCI format 1\_0/1\_1/1\_2 when PDSCH is scheduled with offset equal or larger than the threshold, if applicable.- For FR2 only, aperiodic CSI-RS reception using default beam for enhanced SFN scheme when scheduling offset is less than threshold.The UE indicating support of this feature shall also indicate *sfn-schemeA-r17* or *sfn-schemeB-r17.* | Band | No | N/A | N/A |
| ***sfn-DefaultUL-BeamSetup-r17***Indicates whether the UE supports the following features:- Support of single-TRP PUCCH transmission using default beam when enhanced SFN PDCCH transmission scheme is configured.- Support of single-TRP PUSCH transmission using default beam when enhanced SFN PDCCH transmission scheme is configured.- Support of single-TRP SRS resource transmission using default beam when enhanced SFN PDCCH transmission scheme is configured.The UE indicating support of this feature shall also indicate *sfn-schemeA-r17* or *sfn-schemeB-r17* or *sfn-SchemeA-PDCCH-only-r17*. | Band | No | N/A | FR2 only |
| ***sfn-ImplicitRS-twoTCI-r17***Indicates whether the UE supports RS(s) with two TCI states configured implicitly for beam failure detection enhancement for HST. | Band | No | N/A | N/A |
| ***sfn-QCL-TypeD-Collision-twoTCI-r17***Indicates whether the UE supports identification of two QCL-TypeD properties for multiple overlapping CORESETs when a CORESET is activated with two TCI states which overlaps with another CORESET. | Band | No | N/A | N/A |
| ***simul-SpatialRelationUpdatePUCCHResGroup-r16***Indicates whether the UE support PUCCH resource groups per BWP for simultaneous spatial relation update. The UE indicating support of this also indicates the capabilities of supported SRS resources and maximum supported spatial relations for the supported bands using *supportedSRS-Resources, maxNumberConfiguredSpatialRelations* and *pucch-SpatialRelInfoMAC-CE*. | Band | No | N/A | N/A |
| ***simulTX-SRS-AntSwitchingIntraBandUL-CA-r16***Indicates whether the UE support simultaneous transmission of SRS on different CCs for intra-band UL CA. The UE indicating support of this feature shall include at least one of the following capabilities:- *supportSRS-xTyR-xLessThanY-r16* indicates support transmission of SRS for xTyR (x<y) based antenna switching and SRS for CB/NCB/BM on different CCs in overlapped symbol(s) for intra-band UL CA.- *supportSRS-xTyR-xEqualToY-r16* indicates support transmission of SRS for xTyR (x=y) based antenna switching and SRS for CB/NCB/BM on different CCs in overlapped symbol(s) for intra-band UL CA.- *supportSRS-AntennaSwitching-r16* Indicates whether the UE support simultaneous transmission of SRS for antenna switching on different CCs in overlapped symbol(s) for intra-band UL CA.NOTE: For simultaneously antenna switching and antenna switching SRS in intra-band CAs with bands whose UL are switched together according to the reported *supportSRS-AntennaSwitching-r16*, the UE expects the same configuration of xTyR across the different CCs and the SRS resources overlapped in time domain from UE perspective are from the same UE antenna ports. | Band | No | N/A | N/A |
| ***simulSRS-MIMO-TransWithinBand-r16***Indicates the number of SRS resources for positioning and SRS resource for MIMO on a symbol within a band across multiple CCs. The UE can include this field only if the UE supports *srs-PosResources-r16*. Otherwise, the UE does not include this field. | Band | No | N/A | N/A |
| ***simulSRS-TransWithinBand-r16***Indicates the number of SRS resources for positioning on a symbol within a band across multiple CCs. The UE can include this field only if the UE supports *srs-PosResources-r16*. Otherwise, the UE does not include this field. | Band | No | N/A | N/A |
| ***simultaneousReceptionDiffTypeD-r16***Indicates whether the UE supports simultaneous reception with different QCL Type D reference signal as specified in TS38.213 [11]. | Band | No | N/A | FR2 only |
| ***sn-InitiatedCondPSCellChangeNRDC-r17***Indicates whether the UE supports SN initiated inter-SN conditional PSCell change in NR-DC, which is configured by NR *conditionalReconfiguration* using SN configured measurement as triggering condition. The UE supporting this feature shall also support 2 trigger events for same execution condition in SN initiated inter-SN conditional PSCell change in NR-DC. UE shall set the capability value consistently for all FDD-FR1 bands, all TDD-FR1 bands and all TDD-FR2 bands respectively. | Band | No | N/A | N/A |
| ***spatialRelations, spatialRelations-v1640***Indicates whether the UE supports spatial relations. The capability signalling comprises the following parameters.- *maxNumberConfiguredSpatialRelations* indicates the maximum number of configured spatial relations per CC for PUCCH and SRS. It is not applicable to FR1 and applicable to FR2 only. The UE is mandated to report 16 or higher values. *maxNumberConfiguredSpatialRelations-v1640* indicates the maximum number of configured spatial relations per CC for PUCCH and SRS with UE supporting the configuration of maximum 64 PUCCH spatial relations per BWP per CC;- *maxNumberActiveSpatialRelations* indicates the maximum number of active spatial relations with regarding to PUCCH and SRS for PUSCH, per BWP per CC. It is not applicable to FR1 and applicable and mandatory to report one or higher value for FR2 only;- *additionalActiveSpatialRelationPUCCH* indicates support of one additional active spatial relation for PUCCH. It is mandatory with capability signalling if *maxNumberActiveSpatialRelations* is set to n1;- *maxNumberDL-RS-QCL-TypeD* indicates the maximum number of downlink RS resources used for QCL type D in the active TCI states and active spatial relation information, which is optional.The UE is mandated to report *spatialRelations* for FR2. if *maxNumberConfiguredSpatialRelations-v1640* is reported, UE shall report value *n96* in *maxNumberConfiguredSpatialRelations*. | Band | FD | N/A | FD |
| ***spatialRelationsSRS-Pos-r16***Indicates whether the UE supports spatial relations for SRS for positioning. The capability signalling comprises the following parameters.- *spatialRelation-SRS-PosBasedOnSSB-Serving-r16* indicates whether the UE supports spatial relation for SRS for positioning based on SSB from the serving cell in the same band. The UE can include this field only if the UE supports *srs-PosResources-r16*. Otherwise, the UE does not include this field;- *spatialRelation-SRS-PosBasedOnCSI-RS-Serving-r16* indicates whether the UE supports spatial relation for SRS for positioning based on CSI-RS from the serving cell in the same band. The UE can include this field only if the UE supports *spatialRelation-SRS-PosBasedOnSSB-Serving-r16*. Otherwise, the UE does not include this field;- *spatialRelation-SRS-PosBasedOnPRS-Serving-r16* indicates whether the UE supports spatial relation for SRS for positioning based on PRS from the serving cell in the same band. The UE can include this field only if the UE supports any of DL PRS Resources for DL AoD, DL PRS Resources for DL-TDOA or DL PRS Resources for Multi-RTT defined in TS37.355 [22], or *srs-PosResources-r16*. Otherwise, the UE does not include this field;- *spatialRelation-SRS-PosBasedOnSRS-r16* indicates whether the UE supports spatial relation for SRS for positioning based on SRS in the same band. The UE can include this field only if the UE supports *srs-PosResources-r16*. Otherwise, the UE does not include this field;- *spatialRelation-SRS-PosBasedOnSSB-Neigh-r16* indicates whether the UE supports spatial relation for SRS for positioning based on SSB from the neighbouring cell in the same band. The UE can include this field only if the UE supports *spatialRelation-SRS-PosBasedOnSSB-Serving-r16*. Otherwise, the UE does not include this field;- *spatialRelation-SRS-PosBasedOnPRS-Neigh-r16* indicates whether the UE supports spatial relation for SRS for positioning based on PRS from the neighbouring cell in the same band. The UE can include this field only if the UE supports *spatialRelation-SRS-PosBasedOnPRS-Serving-r16*. Otherwise, the UE does not include this field;NOTE: A PRS from a PRS-only TP is treated as PRS from a non-serving cell. | Band | No | N/A | FR2 only |
| ***spatialRelationsSRS-PosRRC-Inactive-r17***Indicates whether the UE supports spatial relations for SRS for positioning in RRC\_INACTIVE. The capability signalling comprises the following parameters:- *spatialRelation-SRS-PosBasedOnSSB-Serving-r16* indicates whether the UE supports spatial relation for SRS for positioning based on SSB from the serving cell in the same band. The UE indicating support of this feature shall also indicate support of *srs-PosResourcesRRC-Inactive-r17*;- *spatialRelation-SRS-PosBasedOnCSI-RS-Serving-r16* indicates whether the UE supports spatial relation for SRS for positioning based on CSI-RS from the serving cell in the same band. The UE indicating support of this feature shall also indicate support of *spatialRelation-SRS-PosBasedOnSSB-Serving-r16*;- *spatialRelation-SRS-PosBasedOnPRS-Serving-r16* indicates whether the UE supports spatial relation for SRS for positioning based on PRS from the serving cell in the same band. The UE indicating support of this feature shall also indicate support any of DL PRS Resources for DL AoD, DL PRS Resources for DL-TDOA or DL PRS Resources for Multi-RTT defined in TS37.355 [22], or *srs-PosResourcesRRC-Inactive-r17*;- *spatialRelation-SRS-PosBasedOnSRS-r16* indicates whether the UE supports spatial relation for SRS for positioning based on SRS in the same band. The UE indicating support of this feature shall also indicate support of *srs-PosResourcesRRC-Inactive-r17*;- *spatialRelation-SRS-PosBasedOnSSB-Neigh-r16* indicates whether the UE supports spatial relation for SRS for positioning based on SSB from the neighbouring cell in the same band. The UE indicating support of this feature shall also indicate support of *spatialRelation-SRS-PosBasedOnSSB-Serving-r16*;- *spatialRelation-SRS-PosBasedOnPRS-Neigh-r16* indicates whether the UE supports spatial relation for SRS for positioning based on PRS from the neighbouring cell in the same band. The UE indicating support of this feature shall also indicate support of *spatialRelation-SRS-PosBasedOnPRS-Serving-r16*.NOTE: A PRS from a PRS-only TP is treated as PRS from a non-serving cell. | Band | No | N/A | FR2 only |
| ***sp-BeamReportPUCCH***Indicates support of semi-persistent 'CRI/RSRP' or 'SSBRI/RSRP' reporting using PUCCH formats 2, 3 and 4 in one slot. | Band | No | N/A | N/A |
| ***sp-BeamReportPUSCH***Indicates support of semi-persistent 'CRI/RSRP' or 'SSBRI/RSRP' reporting on PUSCH. | Band | No | N/A | N/A |
| ***sps-r16***Indicates whether the UE support of up to 8 configured SPS configurations in a BWP of a serving cell and up to 32 configured SPS configurations in a cell group. This field includes the following parameters:- *maxNumberConfigsPerBWP-r16* indicates the maximum number of active SPS configurations in a BWP of a serving cell.- *maxNumberConfigsAllCC-r16* indicates the maximum number of active SPS configurations across all serving cells in a MAC entity, and across MCG and SCG in case of NR-DC.The UE can include this feature only if the UE indicates support of *downlinkSPS*.NOTE:- For all the reported bands in FR1, a same X1 value is reported for *maxNumberConfigsAllCC-r16*. For all the reported bands in FR2, a same X2 value is reported for *maxNumberConfigsAllCC-r16*.- The total number of active SPS configurations across all serving cells in FR1 is no greater than X1.- The total number of active SPS configurations across all serving cells in FR2 is no greater than X2.- If the CA have some serving cell(s) in FR1 and some serving cell(s) in FR2, the total number of active SPS configurations across all serving cells is no greater than max(X1, X2). | Band | No | N/A | N/A |
| ***srs-AssocCSI-RS***Parameters for the calculation of the precoder for SRS transmission based on channel measurements using associated NZP CSI-RS resource (srs-AssocCSI-RS) as described in clause 6.1.1.2 of TS 38.214 [12]. UE supporting this feature shall also indicate support of non-codebook based PUSCH transmission.This capability signalling includes list of the following parameters:- *maxNumberTxPortsPerResource* indicates the maximum number of Tx ports in a resource;- *maxNumberResourcesPerBand* indicates the maximum number of resources across all CCs within a band simultaneously;*-* *totalNumberTxPortsPerBand* indicates the total number of Tx ports across all CCs within a band simultaneously. | Band | No | N/A | N/A |
| ***srs-combEight-r17***Indicates whether the UE supports comb-8 for SRS other than for positioning. | Band | No | N/A | N/A |
| ***srs-increasedRepetition-r17***Indicates whether the UE supports increased repetition patterns (8, 10, 12, 14 symbols) for SRS resource.The UE supporting this feature shall also indicate the support of *srs-StartAnyOFDM-Symbol-r16*. | Band | No | N/A | N/A |
| ***srs-partialFreqSounding-r17***Indicates the support of partial frequency sounding for SRS for non-frequency hopping case.The UE indicating support of this feature shall also indicate the support of *srs-partialFrequencySounding-r17*. | Band | No | N/A | N/A |
| ***srs-partialFrequencySounding-r17***Indicates whether the UE supports partial frequency sounding for SRS with frequency hopping. | Band | No | N/A | N/A |
| ***srs-PosResourcesRRC-Inactive-r17***Indicates support of positioning SRS transmission in RRC\_INACTIVE for initial UL BWP. The capability signalling comprises the following parameters:- *maxNumberSRS-PosResourceSetPerBWP-r17* Indicates the max number of SRS Resource Sets for positioning supported by UE*;*- *maxNumberSRS-PosResourcesPerBWP-r17* indicates the max number of P/SP SRS Resources for positioning;- *maxNumberSRS-ResourcesPerBWP-PerSlot-r17* indicates the max number of P/SP SRS Resources for positioning per slot;- *maxNumberPeriodicSRS-PosResourcesPerBWP-r17* indicates the max number of periodic SRS Resources for positioning;- *maxNumberPeriodicSRS-PosResourcesPerBWP-PerSlot-r17* indicates the max number of periodic SRS Resources for positioning per slot.NOTE: OLPC for SRS for positioning based on SSB from the last serving cell (the cell that releases UE from connection) is part of this feature. No dedicated capability signalling is intended for this component | Band | No | N/A | N/A |
| ***srs-SemiPersistent-PosResourcesRRC-Inactive-r17***Indicates support of positioning SRS transmission in RRC\_INACTIVE for initial UL BWP with semi-persistent SRS. UE indicating support of this feature shall indicate support of *srs-PosResourcesRRC-Inactive-r17*.The capability signalling comprises the following parameters:- *maxNumOfSemiPersistentSRSposResources-r17* indicates the max number of semi-persistent SRS Resources for positioning;- *maxNumOfSemiPersistentSRSposResourcesPerSlot-r17* indicates the max number of semi-persistent SRS Resources for positioning per slot. | Band | No | N/A | N/A |
| ***srs-PortReport-r17***Indicates the maximum number of SRS ports for each UE reported quantity in *reportQuantity-r17*. | Band | No | N/A | N/A |
| ***srs-PortReportSP-AP-r17***Indicates that the UE supports the maximum number of SRS ports with semi-persistent/aperiodic capability value reporting.The UE supporting this feature shall also indicate support of *srs-PortReport-r17* and one of *aperiodicBeamReport*, *sp-BeamReportPUCCH*, *sp-BeamReportPUSCH,* *ssb-csirs-SINR-measurement-r16, semi-PersistentL1-SINR-Report-PUCCH-r16* or *semi-PersistentL1-SINR-Report-PUSCH-r16.*   | Band | No | N/A | N/A |
| ***srs-startRB-locationHoppingPartial-r17***Indicates whether the UE supports start RB location hopping in partial frequency SRS transmission across different SRS frequency hopping periods for periodic/semi-persistent/aperiodic SRS.The UE supporting this feature shall also indicate the support of *srs-partialFrequencySounding-r17.* | Band | No | N/A | N/A |
| ***srs-TriggeringOffset-r17***Indicates the maximum number of configured available slots offsets for determining aperiodic SRS location based on available slot. | Band | No | N/A | N/A |
| ***srs-TriggeringDCI-r17***Indicates whether the UE supports triggering SRS in DCI 0\_1/0\_2 without data and without CSI. | Band | No | N/A | N/A |
| ***ssb-csirs-SINR-measurement-r16***Indicates the limitations of the UE support of SSB/CSI-RS for L1-SINR measurement.This capability signalling includes list of the following parameters:Per slot limitations:- *maxNumberSSB-CSIRS-OneTx-CMR-r16* indicates the maximum number of SSB/CSI-RS (1TX) across all CCs within a band for Channel Measurement Report- *maxNumberCSI-IM-NZP-IMR-res-r16* indicates the maximum number of CSI-IM/NZP-IMR resources across all CCs within a band- maxNumberCSIRS-2Tx-res-r16 indicates the maximum number of CSI-RS (2TX) resources across all CCs within a band for Channel Measurement ReportMemory limitations:- *maxNumberSSB-CSIRS-res-r16* indicates the max number of SSB/CSI-RS resources across all CCs within a band as Channel Measurement Report- *maxNumberCSI-IM-NZP-IMR-res-mem-r16* indicates the maximum number of CSI-IM/NZP-IMR resources across all CCs within a bandOther limitations:- *supportedCSI-RS-Density-CMR-r16* indicates supported density of CSI-RS for Channel Measurement Report.- *maxNumberAperiodicCSI-RS-Res-r16* indicates the maximum number of aperiodic CSI-RS resources across all CCs within a band configured to measure L1-SINR (including CMR and IMR)- *supportedSINR-meas* indicates the supported SINR measurements.- *supportedSINR-meas-r16* contains values {*ssbWithCSI-IM*, *ssbWithNZP-IMR*, *csirsWithNZP-IMR*, *csi-RSWithoutIMR*} representing {SSB as CMR with dedicated CSI-IM, SSB as CMR with dedicated NZP IMR, CSI-RS as CMR with dedicated NZP IMR configured, CSI-RS as CMR without dedicated IMR configured}.- *supportedSINR-meas-v1670* indicates a 4-bit bitmap {ssbWithCSI-IM, ssbWithNZP-IMR, csirsWithNZP-IMR, csi-RSWithoutIMR}, where the leftmost bit corresponds to ssbWithCSI-IM, the next bit corresponds to ssbWithNZP-IMR and so on. UE indicating *supportedSINR-meas-v1670* shall always indicate *supportedSINR-meas-r16.*UE supporting this feature shall also indicate support of CSI-RS as CMR with dedicated CSI-IM. UE indicating support of this feature shall also indicate support of *periodicBeamReport* and *aperiodicBeamReport* or *sp-BeamReportPUCCH* and *sp-BeamReportPUSCH.* UE indicating support of *ssb-csirs-SINR-measurement-r16* shall support periodic and aperiodic L1-SINR report.NOTE 1: The reference slot duration is the shortest slot duration defined for the frequency range where the reported band belongs.NOTE 2: For *maxNumberSSB-CSIRS-res-r16* and *maxNumberCSI-IM-NZP-IMR-res-mem-r16* the configured CSI-RS resources for both active and inactive BWPs are counted.NOTE 3: For *maxNumberSSB-CSIRS-OneTx-CMR-r16, maxNumberCSI-IM-NZP-IMR-res-r16* and *maxNumberCSIRS-2Tx-res-r16*, CSI-RS resources configured as CMR without dedicated IMR are counted both as CMR and IMR.NOTE 4: For *maxNumberSSB-CSIRS-OneTx-CMR-r16*, *maxNumberCSI-IM-NZP-IMR-res-r16*, *maxNumberCSIRS-2Tx-res-r16*, *maxNumberAperiodicCSI-RS-Res-r16*, a SSB/CSI-RS resource is counted within the duration of a reference slot in which the corresponding reference signals are transmitted.NOTE 5: For *maxNumberSSB-CSIRS-OneTx-CMR-r16*, *maxNumberCSI-IM-NZP-IMR-res-r16*, *maxNumberCSIRS-2Tx-res-r16*, *maxNumberAperiodicCSI-RS-Res-r16*, if one resource used for L1-SINR measurement is referred N times by one or more CSI reporting settings with *reportQuantity-r16* = *ssb-Index-SINR-r16* or *cri-SINR-r16*, it is counted N times.NOTE 6: If more than one type of SINR measurement is indicated in *supportedSINR-meas-v1670*, it is left to UE implementation which SINR measurement to indicate in *supportedSINR-meas-r16*. | Band | No | N/A | N/A |
| ***sssg-Switching-1BitInd-r17***Indicates whether the UE supports 1-bit indication of SSSG switching between 2 SSSGs by scheduling DCI, and timer based SSSG switching, if *pdcch-SkippingDurationList* is not configured as specified in TS 38.213 [11], clause 10.4. UE supports search space set group switching capability-1 according to Table 10.4-1 of TS 38.213 [11]. | Band | No | N/A | N/A |
| ***sssg-Switching-2BitInd-r17***Indicates whether the UE supports 2-bit indication of SSSG switching among 3 SSSGs by scheduling DCI and timer based SSSG switching, if *pdcch-SkippingDurationList* is not configured as specified in TS 38.213 [11], clause 10.4. UE supports search space set group switching capability-1 according to Table 10.4-1 of TS 38.213 [11].UE indicating support of this feature shall also indicate support of *sssg-Switching-1bitInd-r17*. | Band | No | N/A | N/A |
| ***support64CandidateBeamRS-BFR-r16***Indicates UE support of configuring maximum 64 candidate beam RSs per BWP per CC. UE indicating support of this feature shall also indicate support of *maxNumberCSI-RS-BFD, maxNumberSSB-BFD* and *maxNumberCSI-RS-SSB-CBD.* | Band | No | N/A | N/A |
| ***supportCodeWordSoftCombining-r16***Indicates whether UE supports codeword soft combining for FDMSchemeB. UE indicates support of this feature depends on whether the *supportFDM-SchemeB-r16* is also supported. | Band | No | N/A | N/A |
| ***supportFDM-SchemeA-r16***Indicates whether UE supports single DCI based FDMSchemeA. | Band | No | N/A | N/A |
| ***supportInter-slotTDM-r16***Indicates whether UE supports single-DCI based inter-slot TDM. This capability signalling includes the following:- *supportRepNumPDSCH-TDRA-r16* indicates support of RepNumR16 in PDSCH-TimeDomainResourceAllocation and the maximum value of RepNumR16- *maxTBS-Size-r16* indicates maximum TBS size.- *maxNumberTCI-states-r16* indicates the maximum number of TCI states. | Band | No | N/A | N/A |
| ***supportNewDMRS-Port-r16***Indicates whether UE supports new DMRS port entry {0,2,3}. UE supports this feature should indicate support *singleDCI-SDM-scheme-r16* for the band. | Band | No | N/A | N/A |
| ***supportRepNumPDSCH-TDRA-DCI-1-2-r17***Indicates support of *repetitionNumber-v1730* in *PDSCH-TimeDomainResourceAllocation* for DCI format 1\_2 and the maximum value of *repetitionNumber-v1730*. | Band | No | N/A | N/A |
| ***supportTDM-SchemeA-r16***Indicates whether UE supports single DCI based TDMSchemeA. The capability signalling includes the maximum TBS size. | Band | No | N/A | N/A |
| ***supportTwoPortDL-PTRS-r16***Indicates whether UE supports 2-port DL PT-RS. UE supports this feature should indicate support *singleDCI-SDM-scheme-r16* for the band. | Band | No | N/A | N/A |
| ***ta-BasedPDC-NTN-SharedSpectrumChAccess-r17***Indicates whether the UE supports propagation delay compensation based on legacy TA procedure for NTN and shared spectrum channel access. | Band | No | N/A | N/A |
| ***tb-ProcessingMultiSlotPUSCH-r17***Indicates whether UE supports TB processing over multi-slot PUSCH for DG and Type 2 CG without repetition in RRC connected mode. | Band | No | N/A | N/A |
| ***tb-ProcessingRepMultiSlotPUSCH-r17***Indicates whether UE supports repetition of TB processing over multi-slot PUSCH in RRC connected mode.UE supporting this feature shall also indicates support of *tb-ProcessingMultiSlotPUSCH-r17*. | Band | No | N/A | N/A |
| ***tci-StatePDSCH***Defines support of TCI-States for PDSCH. The capability signalling comprises the following parameters:- *maxNumberConfiguredTCIstatesPerCC* indicates the maximum number of configured TCI-states per CC for PDSCH. For FR2, the UE is mandated to set the value at least to 64 (i.e. value 128 is an optional value). For FR1, the UE is mandated to set these values at least to the maximum number of allowed SSBs in the supported band;- *maxNumberActiveTCI-PerBWP* indicates the maximum number of activated TCI-states per BWP per CC, including control and data. If a UE reports X active TCI state(s), it is not expected that more than X active QCL type D assumption(s) for any PDSCH and any CORESETs for a given BWP of a serving cell become active for the UE. The UE shall include this field.Note the UE is required to track only the active TCI states.The UE is mandated to report *tci-StatePDSCH*. | Band | Yes | N/A | N/A |
| ***timeBasedCondHandover-r17***Indicates whether the UE supports time based conditional handover, i.e., *CondEvent T1* as specified in TS 38.331 [9]. A UE supporting this feature shall also indicate the support of *condHandover-r16* for NTN bands and the support of *nonTerrestrialNetwork-r17*. UE shall set the capability value consistently for all FDD-FR1 NTN bands. | Band | No | N/A | N/A |
| ***triggeredHARQ-CodebookRetx-r17***Indicates whether the UE supports triggered HARQ-ACK codebook re-transmission from an earlier PUCCH slot based on the triggering information in DCI format 1\_1 and DCI format 1\_2 (for a UE supporting DCI format 1\_2 as indicated in dci-Format1-2And0-2-r16) and support the related PHY priority handling in terms of HARQ-ACK codebook selection and the applicable PUCCH configuration (for a UE supporting two HARQ-ACK codebooks / PUCCH config as indicated in twoHARQ-ACK-Codebook-type1-r16). The capability signalling comprises the following parameters:- *minHARQ-Retx-Offset-r17* indicates minimum value for the HARQ re-tx offset. Value *n-7* corresponds to -7, value *n-5* corresponds to -5, and so on.- *maxHARQ-Retx-Offset-r17* indicates maximum value for the HARQ re-tx offset.NOTE: The minimum requirement for *minHARQ-Retx-Offset-r17* and *maxHARQ-Retx-Offset-r17* is valid for HARQ CBs consisted of HARQ Processes with a single HARQ bit per HARQ Process ID. | Band | No | N/A | N/A |
| ***trs-AdditionalBandwidth-r16***Indicates the UE supported TRS bandwidths, in addition to 52 RBs, for a 10MHz UE channel bandwidth. This field only applies for the BWPs configured with 52 RBs size and 15kHz SCS, in FDD bands.Value *trs-AddBW-Set1* indicates 28, 32, 36, 40, 44, 48 RBs.Value *trs-AddBW-Set2* indicates 32, 36, 40, 44, 48 RBs. | Band | No | FDD only | FR1 only |
| ***twoPortsPTRS-UL***Defines whether UE supports PT-RS with 2 antenna ports for UL transmission. | Band | No | N/A | N/A |
| ***type1-HARQ-Codebook-r17***Indicates whether the UE supports Type-1 HARQ codebook enhancements when there are feedback-disabled HARQ processes*.* UE indicating support of this feature shall also indicate support of *harq-FeedbackDisabled-r17.* This field is only applicable for bands in Table 5.2.2-1 in TS 38.101-5 [34] and HAPS operation bands in clause 5.2 of TS 38.104 [35]. | Band | No | N/A | N/A |
| ***type2-HARQ-Codebook-r17***Indicates whether the UE supports Type-2 HARQ codebook enhancements when there are feedback-disabled HARQ processes*.* UE indicating support of this feature shall also indicate support of *harq-FeedbackDisabled-r17.* This field is only applicable for bands in Table 5.2.2-1 in TS 38.101-5 [34] and HAPS operation bands in clause 5.2 of TS 38.104 [35]. | Band | No | N/A | N/A |
| ***type1-PUSCH-RepetitionMultiSlots-v1650***Indicates whether the UE supports Type 1 PUSCH transmissions with configured grant as specified in TS 38.214 [12] with UL-TWG-repK value equal to 2, 4, or 8 with a single repetition of the transport block within each slot, and redundancy version pattern as indicated by UL-TWG-RV-rep. A UE supporting this feature shall also support Type 1 PUSCH transmissions with configured grant as specified in TS 38.214 [12] with UL-TWG-repK value of one. This applies only to non-shared spectrum channel access. For shared spectrum channel access, *type1-PUSCH-RepetitionMultiSlots-r16* applies. UE shall set the capability value consistently for all FDD-FR1 bands, all TDD-FR1 bands, all TDD-FR2-1 bands and all TDD-FR2-2 bands respectively.The UE only includes *type1-PUSCH-RepetitionMultiSlots-v1650* if *type1-PUSCH-RepetitionMultiSlots* is absent | Band | No | N/A | N/A |
| ***type2-PUSCH-RepetitionMultiSlots-v1650***Indicates whether the UE supports Type 2 PUSCH transmissions with configured grant as specified in TS 38.214 [12] with UL-TWG-repK value equal to 2, 4, or 8 with a single repetition of the transport block within each slot, and redundancy version pattern as indicated by UL-TWG-RV-rep. A UE supporting this feature shall also support Type 2 PUSCH transmissions with configured grant as specified in TS 38.214 [12] with UL-TWG-repK value of one. This applies only to non-shared spectrum channel access. For shared spectrum channel access, *type2-PUSCH-RepetitionMultiSlots-r16* applies. UE shall set the capability value consistently for all FDD-FR1 bands, all TDD-FR1 bands, all TDD-FR2-1 bands and all TDD-FR2-2 bands respectively.The UE only includes *type2-PUSCH-RepetitionMultiSlots-v1650* if *type2-PUSCH-RepetitionMultiSlots* is absent | Band | No | N/A | N/A |
| ***type3-HARQ-Codebook-r17***Indicates whether the UE supports Type-3 HARQ codebook enhancements when there are feedback-disabled HARQ processes*.* UE indicating support of this feature shall also indicate support of *harq-FeedbackDisabled-r17.* This field is only applicable for bands in Table 5.2.2-1 in TS 38.101-5 [34] and HAPS operation bands in clause 5.2 of TS 38.104 [35]. | Band | No | N/A | N/A |
| ***txDiversity-r16***Indicates whether the UE supports transparent Tx diversity requirements as specified in the suffix G clauses of TS 38.101-1 [2] (see also clauses 4.2 and 4.3 of TS38.101-1 [2]). | Band | No | N/A | FR1 only |
| ***ue-OneShotUL-TimingAdj-r17***Indicates whether the UE supports one shot large UL timing adjustment.UE indicating support of this feature shall indicate support of *ue-PowerClass-v1700* set to *'pc6'.* | Band | No | N/A | FR2 only |
| ***ue-PowerClass, ue-PowerClass-v1610, ue-PowerClass-v1700***For FR1, if the UE supports the different UE power class than the default UE power class as defined in clause 6.2 of TS 38.101-1 [2], the UE shall report the supported UE power class in this field. For FR2, UE shall report the supported UE power class as defined in clause 6 and 7 of TS 38.101-2 [3] in this field. UE indicating support for *pc6* supports the enhanced intra-NR RRM and demodulation processing requirements for FR2 to support high speed up to 350 km/h as specified in TS 38.133 [5]. This capability is not applicable to IAB-MT. The power class pc7 is only applicable for RedCap UEs operation in FR2. | Band | Yes | N/A | N/A |
| ***ue-specific-K-Offset-r17***Indicates whether the UE supports the reception of UE-specific K\_offset comprised of the following functional components:- Support of reception of UE-specific K\_offset via MAC-CE- Support of determining the timing of PUSCH, PUCCH, CSI reference resource, transmission of aperiodic SRS, activation of TA command, first PUSCH transmission in CG Type 2 with UE-specific KoffsetUE indicating support of this feature shall also indicate support of *uplinkPreCompensation-r17* and *uplink-TA-Reporting-r17* for this band*.* This field is only applicable for bands in Table 5.2.2-1 in TS 38.101-5 [34] and HAPS operation bands in clause 5.2 of TS 38.104 [35]. | Band | No | N/A | N/A |
| ***ul-GapFR2-r17***Indicates whether the UE supports FR2 UL gap to perform BPS sensing for Tx power management by the use of uplink gap patterns as specified in TS 38.133 [5] if UE supports a band in FR2. | Band | No | No | FR2 only |
| ***unifiedJointTCI-BeamAlignDLRS-r17***Indicates the support of beam misalignment between the DL source RS in the TCI state to provide spatial relation indication and the PL-RS.The UE indicating support of this feature shall also indicate support of *unifiedJointTCI-r17*. | Band | No | N/A | FR2 only |
| ***unifiedJointTCI-commonMultiCC-r17***Indicates the support of common multi-CC TCI state ID update and activation.The UE indicating support of this feature shall also indicate support of *unifiedJointTCI-r17*. | Band | No | N/A | N/A |
| ***unifiedJointTCI-InterCell-r17***Indicates the support of Unified TCI with joint DL/UL TCI update for inter-cell beam management including following parameters:- *additionalMAC-CE-PerCC-r17* indicates the number of K additional MAC-CEs to indicate joint TCI states per CC in a band.- *additionalMAC-CE-AcrossCC-r17* indicates the number of K additional MAC-CE activated joint TCI states across all CC(s) in a band.A UE indicating support of this shall also indicate support of *unifiedJointTCI-r17* and *unifiedJointTCI-mTRP-InterCell-BM-r17*.NOTE: A UE that supports *unifiedJointTCI-InterCell-r17* supports K additional MAC-CE activated joint TCI states across all CC(s) in a band in addition to the maximum number of MAC-CE activated joint TCI states across all CC(s) in a band signalled in *unifiedJointTCI-r17*. The signalled value in *additionalMAC-CE-AcrossCC-r17* plus the signalled value in *maxActivatedTCIAcrossCC-r17* determine the maximum number of MAC-CE activated joint TCI states across all CC(s) in a band that are applied to intra and inter-cell beam management jointly. | Band | No | N/A | N/A |
| ***unifiedJointTCI-Legacy-CORESET0-r17*** Indicates the support of indication/configuration of R17 TCI states for CORESET #0 and the respective PDSCH reception reusing the Rel-15/16 signalling/configuration design(s)***.***The UE indicating support of this feature shall also indicate support of *unifiedJointTCI-r17*. | Band | No | N/A | N/A |
| ***unifiedJointTCI-Legacy-SRS-r17***Indicates the support of indication/configuration of R17 TCI states for SRS (except for periodic/semi-persistent SRS for BM) reusing the Rel-15/16 signalling/configuration design(s).The UE indicating support of this feature shall also indicate support of *unifiedJointTCI-r17*. | Band | No | N/A | N/A |
| ***unifiedJointTCI-Legacy-r17***Indicates the support of indication/configuration of R17 TCI states for aperiodic CSI-RS, PDCCH, PDSCH (except for TRS and for CORESET #0 and the respective PDSCH reception) reusing the Rel-15/16 signalling/configuration design(s).The UE indicating support of this feature shall also indicate support of *unifiedJointTCI-r17*. | Band | No | N/A | N/A |
| ***unifiedJointTCI-ListSharingCA-r17***Indicates the support of reference BWP/serving cell index to indicate reference TCI state list shared by multiple BWPs/serving cells. The value indicates the maximum number of configured joint TCI state lists across all BWPs and all Serving cells in a band.The UE indicating support of this feature shall also indicate support of *unifiedJointTCI-r17*. A UE that supports CA and *unifiedJointTCI-r17* shall indicate support of this feature. | Band | No | N/A | N/A |
| ***unifiedJointTCI-mTRP-InterCell-BM-r17***Indicates the support of inter-cell beam measurement and reporting for inter-cell BM and mTRP. This feature includes support of L1-RSRP measurement and reporting on SSB(s) with PCI(s) different from serving cell PCI (additional PCI) and support of up to K SSBRI-RSRP pairs in one report where a pair is associated with a PCI different from serving cell PCI can be reported, where K is equal to *maxNumberNonGroupBeamReporting*.This feature also includes following parameters:- *maxNumAdditionalPCI-L1-RSRP-r17* indicates the maximum number of RRC-configured] PCI(s) different from serving cell PCI for L1-RSRP measurement.- *maxNumSSB-ResourceL1-RSRP-AcrossCC-r17* indicates the maximum number of SSB resources configured to measure L1-RSRP within a slot with PCI(s) same as or different from serving cell PCI [across all CC].NOTE: *maxNumSSBResource-L1-RSRP-AcrossCC-r17* is also counted in *maxTotalResourcesForOneFreqRange-r16/ maxTotalResourcesForAcrossFreqRanges-r16*. | Band | No | N/A | N/A |
| ***unifiedJointTCI-multiMAC-CE-r17***Indicates the support of unified TCI state operation with joint DL/UL TCI update for intra- and inter-cell beam management with more than one MAC-CE activated joint TCI state per CC with MAC CE and DCI based TCI state indication in DCI formats 1\_1 and 1\_2 with and without DL assignment.This capability signalling includes the following parameters:- *minBeamApplicationTime-r17* indicates the minimum beam application time in Y symbols per SCS indicated only for FR2.- *maxNumMAC-CE-PerCC-r17* indicates the maximum number of MAC-CE activated joint TCI states per CC in a band.The UE indicating support of this feature shall also indicate support of *unifiedJointTCI-r17*.NOTE 1: The maximum number of MAC-CE activated joint TCI states across all CC(s) in a band for more than one MAC-CE activated joint TCI state is signaled in *unifiedJointTCI-r17.*NOTE 2: Activated joint TCI state(s) include all PDCCH/PDSCH receptions and PUSCH/PUCCH. | Band | No | N/A | N/A |
| ***unifiedJointTCI-PC-association-r17***Indicates the support of association between TCI state and UL PC settings except for PL RSfor PUCCH, PUSCH, and SRS.The UE indicating support of this feature shall also indicate support of *unifiedJointTCI-r17*. | Band | No | N/A | N/A |
| ***unifiedJointTCI-perBWP-CA-r17***Indicates the support of TCI state list configuration per BWP when CA is configured.The UE indicating support of this feature shall also indicate support of *unifiedJointTCI-r17*. | Band | No | N/A | N/A |
| ***unifiedJointTCI-r17***Indicates the support of unified TCI state operation with joint DL/UL TCI update for intra-cell beam management including the support of:- One MAC-CE activated joint TCI state per CC in a band- TCI state indication for update and activation of MAC CE based TCI state indication for one active TCI stateThe capability signalling comprises the following parameters:- *maxConfiguredJointTCI-r17* indicates the maximum number of configured joint TCI states per BWP per CC in a band- *maxActivatedTCIAcrossCC-r1*7 indicates the maximum number of MAC-CE activated joint TCI states across all CC(s) in a bandIf a UE supports *unifiedJointTCI-InterCell-r17*, the signalled component values (except *additionalMAC-CE-AcrossCC-r17*) also apply to inter-cell beam management,NOTE: Activated joint TCI state(s) include all PDCCH/PDSCH receptions and PUSCH/PUCCH transmissions | Band | No | N/A | N/A |
| ***unifiedJointTCI-SCellBFR-r17***Indicates the support of SCell BFR with unified TCI operation. The maximum number of CCs configured with SCell BFR with unified TCI framework in a band with SpCell BFR is given by *maxNumberSCellBFR-r16*. The UE supporting this feature assumes that maxNumberSCellBFR-r16 includes SpCell. | Band | No | N/A | N/A |
| ***unifiedSeparateTCI-commonMultiCC-r17***Indicates the Common multi-CC DL/UL-TCI state ID update and activation.The UE indicating support of this feature shall also indicate support of *unifiedSeparateTCI-r17*. | Band | No | N/A | N/A |
| ***unifiedSeparateTCI-InterCell-r17***Indicates the support of unified TCI with separate DL/UL TCI update for inter-cell beam management with more than one MAC-CE activated separate TCI state per CC.This feature also includes following parameters:- *k-DL-PerCC-r17* indicates the number of additional MAC-CE activated DL TCI states per CC in a band- *k-UL-PerCC-r17* indicates the number of additional MAC-CE activated UL TCI states per CC in a band- *k-DL-AcrossCC-r17* indicates the number of additional MAC-CE activated DL TCI states across all CC(s) in a band- *k-UL-AcrossCC-r17* indicates the number of additional MAC-CE activated UL TCI states across all CC(s) in a bandThe UE indicating support of this feature shall also indicate support of *unifiedSeparateTCI-r17*.NOTE: A UE that supports this feature supports K additional MAC-CE activated DL and K additional MAC-CE activated UL TCI states across all CC(s) in a band in addition to the maximum number of MAC-CE activated DL and UL TCI states across all CC(s) in a band signalled in *unifiedSeperateTCI-r17*. The signalled value in *k-DL-AcrossCC-r17* (*k-UL-AcrossCC-r17*) plus the signalled value in *maxActivatedDL-TCIAcrossCC-r17* (*maxActivatedUL-TCIAcrossCC-r17*) determine the maximum number of MAC-CE activated DL (UL) TCI states across all CC(s) in a band that are applied to intra and inter-cell beam management jointly. | Band | No | N/A | N/A |
| ***unifiedSeparateTCI-ListSharingCA-r17***Indicates the support of reference BWP/serving cell configured with reference TCI state pool shared by a set of BWPs/serving cells. The value indicates the maximum number of configured DL/UL TCI state pools across all BWPs and all serving cells in a band. | Band | No | N/A | N/A |
| ***unifiedSeparateTCI-multiMAC-CE-r17***Indicates TCI state indication for update and activation a) MAC-CE+DCI-based TCI state indication (use of DCI formats 1\_1/1\_2 with DL assignment)And b) MAC-CE+DCI-based TCI state indication (use of DCI formats 1\_1/1\_2 without DL assignment).This capability signalling includes the following parameters:- *minBeamApplicationTime-r17* indicates the minimum beam application time in Y symbols per SCS.- *maxActivatedDL-TCIPerCC-r17* indicates the maximum number of MAC-CE activated DL TCI states per CC in a band- *maxActivatedUL-TCIPerCC-r17* indicates the maximum number of MAC-CE activated UL TCI states per CC in a bandThe UE indicating support of this feature shall also indicate support of *unifiedSeparateTCI-r17*. | Band | No | N/A | N/A |
| ***unifiedSeparateTCI-perBWP-CA-r17***Indicates the support of DL/UL TCI state pool configuration per BWP for CA mode.The UE indicating support of this feature shall also indicate support of *unifiedSeparateTCI-r17*. | Band | No | N/A | N/A |
| ***unifiedSeparateTCI-r17***Indicates the support of unified TCI state operation with joint DL/UL TCI update for intra-cell beam management including the support of:- One MAC-CE activated DL TCI state per CC in a band- One MAC-CE activated UL TCI state per CC in a band- TCI state indication for update and activation including MAC CE based TCI state indication for one active DL/UL TCI stateThe capability signalling comprises the following parameters:- *maxConfiguredDL-TCI-r17* indicates the maximum number of configured DL TCI states per BWP per CC- *maxConfiguredUL-TCI-r17* indicates the maximum number of configured UL TCI states per BWP per CC- *maxActivatedDL-TCIAcrossCC-r17* indicates the maximum number of MAC-CE activated DL TCI states across all CC(s) in a band- *maxActivatedUL-TCIAcrossCC-r17* indicates the maximum number of MAC-CE activated UL TCI states across all CC(s) in a bandThe UE indicating support of this feature shall also indicate support of *unifiedJointTCI-r17*. If a UE supports *unifiedSeperateTCI-InterCell-r17*, the *maxConfiguredDL-TCI-r17* and *maxConfiguredUL-TCI-r17* apply to intra- and inter-cell beam management jointly. | Band | No | N/A | N/A |
| ***uplinkBeamManagement***Defines support of beam management for UL. This capability signalling comprises the following parameters:- *maxNumberSRS-ResourcePerSet-BM* indicates the maximum number of SRS resources per SRS resource set configurable for beam management, supported by the UE.- *maxNumberSRS-ResourceSet* indicates the maximum number of SRS resource sets configurable for beam management, supported by the UE.If the UE does not set *beamCorrespondenceWithoutUL-BeamSweeping* to *supported*, the UE shall report this capability. This feature is optional for the UE that supports beam correspondence without uplink beam sweeping as defined in clause 6.6, TS 38.101-2 [3].NOTE: The network uses *maxNumberSRS-ResourceSet* to determine the maximum number of SRS resource sets that can be configured to the UE for periodic/semi-persistent/aperiodic configurations as below:

|  |  |
| --- | --- |
| Maximum number of SRS resource sets across all time domain behaviour (periodic/semi-persistent/aperiodic) reported in *maxNumberSRS-ResourceSet* | Additional constraint on the maximum number of SRS resource sets configured to the UE for each supported time domain behaviour (periodic/semi-persistent/aperiodic) |
| 1 | 1 |
| 2 | 1 |
| 3 | 1 |
| 4 | 2 |
| 5 | 2 |
| 6 | 2 |
| 7 | 4 |
| 8 | 4 |

 | Band | No | N/A | FR2 only |
| ***uplinkPreCompensation-r17***Indicates whether the UE supports the uplink time and frequency pre-compensation and timing relationship enhancements comprised of the following functional components:- Support of UE specific TA calculation based on its GNSS-acquired position and the serving satellite ephemeris.- Support of common TA calculation according to the parameters provided by the network (UE considers common TA as 0 if the parameters are not provided)- For TA update in RRC\_CONNECTED state, support of combination of both open (i.e. UE autonomous TA estimation, and common TA estimation) and closed (i.e., received TA commands) control loops- Support of pre-compensation of the calculated TA in its uplink transmissions- Support of estimating UE-gNB RTT and delaying the start of RAR window by UE-gNB RTT- Support of frequency pre-compensation to counter shift the Doppler experienced on the service link- Support of determining timing of the scheduling of PUSCH, PUCCH and PDCCH ordered PRACH, CSI reference resource, transmission of aperiodic SRS activation of TA command, first PUSCH transmission in CG Type 2 with cell-specific K\_offset if indicated- Support of determining timing of the UE action and assumption on a downlink configuration carried by MAC CE command by K\_mac if it is indicated and determining the timing of PDCCH monitoring in recovery search space using K-mac during beam failure recovery procedure- Support of UE receiving cell-specific K\_offset/K\_mac in system informationSupport of this feature in NTN bands is mandatory for UE supporting *nonTerrestrialNetwork-r17*. This field is only applicable for bands in Table 5.2.2-1 in TS 38.101-5 [34] and HAPS operation bands in clause 5.2 of TS 38.104 [35]. | Band | CY | N/A | N/A |
| ***uplink-TA-Reporting-r17***Indicates whether the UE supports UE reporting of information related to TA pre-compensation as specified in TS 38.321 [8]*.* UE indicating support of this feature shall also indicate support of *uplinkPreCompensation-r17* for this band. This field is only applicable for bands in Table 5.2.2-1 in TS 38.101-5 [34] and HAPS operation bands in clause 5.2 of TS 38.104 [35]. | Band | No | N/A | N/A |

|  |
| --- |
| NEXT CHANGE |

#### 4.2.7.5 *FeatureSetDownlink* parameters

| Definitions for parameters | Per | M | FDD-TDDDIFF | FR1-FR2DIFF |
| --- | --- | --- | --- | --- |
| ***additionalDMRS-DL-Alt***Indicates whether the UE supports the alternative additional DMRS position for co-existence with LTE CRS. It is applied to 15kHz SCS and one additional DMRS case only. | FS | No | N/A | FR1 only |
| ***cbgPDSCH-ProcessingType1-DifferentTB-PerSlot-r16***Defines whether the UE capable of processing time capability 1 supports CBG based reception with one or with up to two or with up to four or with up to seven unicast PDSCHs per slot per CC. | FS | No | N/A | N/A |
| ***cbgPDSCH-ProcessingType2-DifferentTB-PerSlot-r16***Defines whether the UE capable of processing time capability 2 supports CBG based reception with one or with up to two or with up to four or with up to seven unicast PDSCHs per slot per CC. | FS | No | N/A | N/A |
| ***crossCarrierSchedulingProcessing-DiffSCS-r16***Indicates the UE cross carrier scheduling processing capability for DL carrier aggregation processing up to X unicast DCI scheduling for DL per scheduled CC. X is based on pair of (scheduling CC SCS, scheduled CC SCS) where a pair of (15,120), (15,60), (30,120) kHz SCS can have X = {1,2,4} while a pair of (15,30), (30,60), (60,120) kHz SCS can have X = {2}, and X applies per slot of scheduling CC. | FS | No | N/A | N/A |
| ***csi-RS-MeasSCellWithoutSSB***Defines whether the UE can perform CSI-RSRP and CSI-RSRQ measurement as specified in TS 38.215 [13], where CSI-RS resource is configured for a cell that does not transmit SS/PBCH block. A UE that supports this feature shall also support scellWithoutSSB. | FS | No | N/A | N/A |
| ***dl-MCS-TableAlt-DynamicIndication***Indicates whether the UE supports dynamic indication of MCS table for PDSCH. | FS | No | N/A | N/A |
| ***dynamicMulticastPCell-r17***Indicates whether the UE supports dynamic scheduling for multicast for PCell comprised of the following functional components:- Supports group-common PDCCH/PDSCH for multicast with CRC scrambled by G-RNTI for PCell;- Supports CFR configuration for multicast;- Supports CORESET and common search space configuration for multicast;- Supports DCI format 4\_1 with CRC scrambled with G-RNTI for multicast;- Supports inter-slot TDM between group-common PDSCH for multicast and other PDSCHs in different slots;- Supports {2, 4, 8} times semi-static slot-level repetition for group-common PDSCH for multicast;- Supports long DRX cycle for MBS multicast reception as specified in TS 38.321 [8]. | FS | No | N/A | N/A |
| ***featureSetListPerDownlinkCC***Indicates which features the UE supports on the individual DL carriers of the feature set (and hence of a band entry that refer to the feature set) by *FeatureSetDownlinkPerCC-Id*. The order of the elements in this list is not relevant, i.e., the network may configure any of the carriers in accordance with any of the *FeatureSetDownlinkPerCC-Id* in this list. A fallback per CC feature set resulting from the reported feature set per DL CC is not signalled but the UE shall support it. | FS | N/A | N/A | N/A |
| ***intraBandFreqSeparationDL, intraBandFreqSeparationDL-v1620***Indicates DL frequency separation class the UE supports, which indicates a maximum frequency separation between lower edge of lowest CC and upper edge of highest CC in a frequency band, for intra-band non-contiguous CA. The UE sets the same value in the FeatureSetDownlink of each band entry within a band. The values mhzX correspond to the values XMHz defined in TS 38.101-2 [3]. It is mandatory to report for UE which supports DL intra-band non-contiguous CA in FR2.If the UE sets the field *intraBandFreqSeparationDL-v1620* it shall set *intraBandFreqSeparationDL* (without suffix) to the nearest smaller value. | FS | CY | N/A | FR2 only |
| ***intraBandFreqSeparationDL-Only-r16***Indicates whether the UE supports frequency separation class of DL only extension. If present, the field extends the maximum frequency separation between the lower edge of lowest CC and the upper edge of highest CC in a frequency band that the UE supports according to *intraBandFreqSeparationDL*.The frequency range extension is either above or below the frequency range indicated by *intraBandFreqSeparationDL* and extends it in contiguous manner with no frequency gap, and the network may configure contiguous or non-contiguous downlink serving cells in that extended range. The UE sets the same value in the FeatureSetDownlink of each band entry within a band. The values mhzX correspond to the values XMHz defined in TS38.101-2 [3]. The sum of *intraBandFreqSeparationDL* and *intraBandFreqSeparationDL-Only* shall not exceed 2400 MHz. If the UE sets this field, the sum of *intraBandFreqSeparationDL* and *intraBandFreqSeparationDL-Only* shall be larger than 1400 MHz.A UE supporting this feature shall also support *intraBandFreqSeparationDL*. | FS | No | N/A | FR2 only |
| ***intraFreqDAPS-r16***Indicates whether UE supports intra-frequency DAPS handover, e.g. support of simultaneous DL reception of PDCCH and PDSCH from source and target cell. A UE indicating this capability shall also support intra-frequency synchronous DAPS handover, single UL transmission and cancelling UL transmission to the source cell for intra-frequency DAPS handover. The capability signalling comprises of the following parameters:- *intraFreqAsyncDAPS-r16* indicates whether the UE supports asynchronous DAPS handover.- *intraFreqDiffSCS-DAPS-r16* indicates whether the UE supports different SCSs in source PCell and intra-frequency target PCell in DAPS handover. The UE only includes this field if different SCSs can be supported in both UL and DL. If absent, the UE does not support either UL or DL SCS being different in DAPS handover. | FS | No | N/A | N/A |
| ***mTRP-PDCCH-Repetition-r17***Indicates the support of intra-slot PDCCH repetition based on two linked SS sets associated with corresponding CORESETs.This feature also includes following parameters:- *numBD-twoPDCCH-r17* indicates the number of BDs for the two PDCCH candidates.- *maxNumOverlaps-r17* indicates the maximum number of overlaps when one of the linked PDCCH candidates uses the same set of CCEs as an individual (unlinked) PDCCH candidate per scheduled component carrier per slot.NOTE 1: UE supports PDCCH repetition for the following (basic) PDCCH monitoring capability: For type 1 CSS with dedicated RRC configuration, type 3 CSS, and UE-SS, the monitoring occasion is within the first 3 OFDM symbols of a slot.NOTE 2: For *maxNumOverlaps-r17*, each unique pair of overlaps is counted as one.NOTE 3: This feature does not include supporting two QCL-TypeD in time-domain overlapping CORESETs in FR2. | FS | No | N/A | N/A |
| ***mTRP-PDCCH-Case2-1SpanGap-r17***Indicates the support of PDCCH repetition for PDCCH monitoring of any occasions with span gap as defined in *pdcch-MonitoringAnyOccasionsWithSpanGap* for each SCS with the following parameters:- *supportedMode-r17* indicates supported mode of PDCCH repetition.- *limitX-PerCC-r17*: limit (X) per CC.- *limitX-AcrossCC-r17*: limit (X) per across all CCs.The limit (X) is the total number of linked candidates of which the first candidate is received and the second one has not been received at any given span, where "received" and "not been received" is with respect to the end of the corresponding span of PDCCH candidate. It is indicated as a total count assuming count 1 for AL=1; 2 for AL=2; 4 for AL=4 or 8 or 16.The UE indicates *limitX-PerCC-r17* and *limitX-AcrossCC-r17* if *supportedMode-r17* is set to *inter-span* or *both*. A candidate value "*nolimit*" does not imply BD limit can be exceeded.The UE indicating support of this feature shall also indicate support of *pdcch-MonitoringAnyOccasionsWithSpanGap* and *mTRP-PDCCH-Repetition-r17*. | FS | No | N/A | N/A |
| ***mTRP-PDCCH-legacyMonitoring-r17***Indicates the support of PDCCH repetition with Rel-16 PDCCH monitoring capability as defined in *pdcch-Monitoring-r16* for 15kHz and 30kHz SCS with the following parameters:- *supportedMode-r17* indicates the supported mode of PDCCH repetition.- *limitX-PerCC-r17* indicates the limit (X) per CC.- *limitX-AcrossCC-r17* indicates the limit (X) per across all CCs.The limit (X) is the total number of linked candidates of which the first candidate is received and the second one has not been received at any given span, where "received" and "not been received" is with respect to the end of the corresponding span of PDCCH candidate. It is indicated as a total count assuming count 1 for AL=1; 2 for AL=2; 4 for AL=4 or 8 or 16.The UE indicates *limitX-PerCC-r17* and *limitX-AcrossCC-r17* if *supportedMode-r17* is set to *inter-span* or *both*. A candidate value "*nolimit*" does not imply BD limit can be exceeded.The UE indicating support of this feature shall also indicate support of *pdcch-Monitoring-r16* and *mTRP-PDCCH-Repetition-r17*. | FS | No | N/A | N/A |
| ***mTRP-PDCCH-multiDCI-multiTRP-r17***Indicates the support of simultaneous configuration of PDCCH repetition and multi-DCI based multi-TRP. Two linked PDCCH candidates are not expected to be associated with different CORESETPoolIndex valuesThe UE indicating support of this feature shall also indicate support of *multiDCI-MultiTRP-r16* and *mTRP-PDCCH-Repetition-r17*. | FS | No | N/A | N/A |
| ***oneFL-DMRS-ThreeAdditionalDMRS-DL***Defines whether the UE supports DM-RS pattern for DL transmission with 1 symbol front-loaded DM-RS with three additional DM-RS symbols. | FS | No | N/A | N/A |
| ***oneFL-DMRS-TwoAdditionalDMRS-DL***Defines support of DM-RS pattern for DL transmission with 1 symbol front-loaded DM-RS with 2 additional DM-RS symbols and more than 1 antenna ports. | FS | Yes | N/A | N/A |
| ***pdcch-Monitoring-r16***Indicates whether the UE supports PDCCH search space monitoring occasions in any symbol of the slot with minimum time separation between two consecutive transmissions of PDCCH with span up to two OFDM symbols for two OFDM symbols or span up to three OFDM symbols for four and seven OFDM symbols. The different value can be reported for PDSCH processing type 1 and PDSCH processing type 2, respectively. For each sub-carrier spacing, the leading / leftmost bit (bit 0) corresponds to the supported value set (X,Y) of (7,3). The next bit (bit 1) corresponds to the supported value set (X,Y) of (4,3). The rightmost bit (bit 2) corresponds to the supported value set (X,Y) of (2,2). | FS | No | N/A | N/A |
| ***pdcch-MonitoringAnyOccasions***Defines the supported PDCCH search space monitoring occasions. withoutDCI-gap indicates whether the UE supports PDCCH search space monitoring occasions in any symbol of the slot for Type 1-PDCCH common search space configured by dedicated RRC signalling, for a Type 3-PDCCH common search space, or for a UE-specific search space with the capability of supporting at least 44, 36, 22, and 20 blind decodes in a slot for 15 kHz, 30 kHz, 60kHz, and 120 kHz subcarrier spacing values respectively. withDCI-gap indicates whether the UE supports PDCCH search space monitoring occasions in any symbol of the slot with minimum time separation of two OFDM symbols for 15 kHz, four OFDM symbols for 30 kHz, seven OFDM symbols for 60 kHz with NCP, and 14OFDM symbols for 120kHz between two consecutive transmissions of PDCCH scrambled with C-RNTI, MCS-C-RNTI, or CS-RNTI for Type 1-PDCCH common search space configured by dedicated RRC signalling, for a Type 3-PDCCH common search space, or for a UE-specific search space, with the capability of supporting at least 44, 36, 22, and 20 blind decodes in a slot for 15 kHz, 30 kHz, 60kHz, and 120 kHz subcarrier spacing values respectively. | FS | No | N/A | N/A |
| ***pdcch-MonitoringAnyOccasionsWithSpanGap***Indicates whether the UE supports PDCCH search space monitoring occasions in any symbol of the slot with minimum time separation between two consecutive transmissions of PDCCH with span up to two OFDM symbols for two OFDM symbols or span up to three OFDM symbols for four and seven OFDM symbols. Value set1 indicates the supported value set (X,Y) is (7,3), value set2 indicates the supported value set (X,Y) is (4,3) and (7,3) and value set 3 indicates the supported value set (X,Y) is (2,2), (4,3) and (7,3). | FS | No | N/A | N/A |
| ***pdcch-MonitoringMixed-r16***Indicates support of Rel-15 monitoring capability and *pdcch-Monitoring-r16* on different serving cells. | FS | No | N/A | N/A |
| ***pdsch-ProcessingType1-DifferentTB-PerSlot***Defines whether the UE capable of processing time capability 1 supports reception of up to two, four or seven unicast PDSCHs for several transport blocks with PDSCH scrambled using C-RNTI, TC-RNTI, MCS-C-RNTI or CS-RNTI in one serving cell within the same slot per CC that are multiplexed in time domain only.NOTE: PDSCH(s) for Msg.4 is included. | FS | No | N/A | N/A |
| ***pdsch-ProcessingType2***Indicates whether the UE supports PDSCH processing capability 2. The UE supports it only if all serving cells are self-scheduled and if all serving cells in one band on which the network configured processingType2 use the same subcarrier spacing. This capability signalling comprises the following parameters for each sub-carrier spacing supported by the UE.- *fallback* indicates whether the UE supports PDSCH processing capability 2 when the number of configured carriers is larger than *numberOfCarriers* for a reported value of *differentTB-PerSlot*. If *fallback* = 'sc', UE supports capability 2 processing time on lowest cell index among the configured carriers in the band where the value is reported, if *fallback* = 'cap1-only', UE supports only capability 1, in the band where the value is reported;- *differentTB-PerSlot* indicates whether the UE supports processing type 2 for 1, 2, 4 and/or 7 unicast PDSCHs for different transport blocks per slot per CC; and if so, it indicates up to which number of CA serving cells the UE supports that number of unicast PDSCHs for different TBs. The UE shall include at least one of *numberOfCarriers* for 1, 2, 4 or 7 transport blocks per slot in this field if *pdsch-ProcessingType2* is indicated. | FS | No | N/A | FR1 only |
| ***pdsch-ProcessingType2-Limited***Indicates whether the UE supports PDSCH processing capability 2 with scheduling limitation for SCS 30kHz. This capability signalling comprises the following parameter.- *differentTB-PerSlot-SCS-30kHz* indicates the number of different TBs per slot.The UE supports this limited processing capability 2 only if:1) One carrier is configured in the band, independent of the number of carriers configured in the other bands;2) The maximum bandwidth of PDSCH is 136 PRBs;3) N1 based on Table 5.3-2 of TS 38.214 [12] for SCS 30 kHz. | FS | No | N/A | FR1 only |
| ***pdsch-SeparationWithGap***Indicates whether the UE supports separation of two unicast PDSCHs with a gap, applicable to Sub-carrier spacings of 30 kHz and 60 kHz only. For any two consecutive slots n and n+1, if there are more than 1 unicast PDSCH in either slot, the minimum time separation between starting time of any two unicast PDSCHs within the duration of these slots is 4 OFDM symbols for 30kHz and 7 OFDM symbols for 60kHz. | FS | No | N/A | N/A |
| ***prs-AsSpatialRelationRS-For-SRS-r17***Indicates whether the UE supports PRS as spatial relation RS for SRS.A UE supporting this feature shall also indicate support of *rtt-BasedPDC-PRS-r17*. | FS | No | N/A | FR2 only |
| ***rtt-BasedPDC-CSI-RS-ForTracking-r17***Indicates whether the UE supports RTT-based propagation delay compensation for time synchronization of the Uu interface based on CSI-RS for tracking and SRS.A UE supporting this feature shall also indicate support of *csi-RS-ForTracking* and *supportedSRS-Resources*. | FS | No | N/A | N/A |
| ***rtt-BasedPDC-PRS-r17***Indicates whether the UE supports RTT-based Propagation delay compensation for time synchronization of the Uu interface based on DL PRS and SRS. The capability signalling comprises the following parameters:- *maxNumberPRS-Resource-r17* indicates the maximum number of DL PRS Resources in DL PRS Resource Set for PDC, with value n16, n32, and n64 only applicable to FR2 bands.- *maxNumberPRS-ResourceProcessedPerSlot-r17* indicates the maximum number of DL PRS resources that UE can process in a slot.A UE supporting this feature shall also indicate support of *supportedSRS-Resources*. | FS | No | N/A | N/A |
| ***scalingFactor***Indicates the scaling factor to be applied to the serving cell in the max data rate calculation when *mcs-Table-r17* and *mcs-TableDCI-1-2-r17* are not configured for the serving cell as defined in 4.1.2. Value f0p4 indicates the scaling factor 0.4, f0p75 indicates 0.75, and so on. If absent, the scaling factor 1 is applied to the band in the max data rate calculation. | FS | No | N/A | N/A |
| ***scalingFactor-1024QAM-FR1-r17***Indicates the scaling factor to be applied to the serving cell in the max data rate calculation when *mcs-Table-r17* or *mcs-TableDCI-1-2-r17* is configured for the serving cell as defined in 4.1.2 when support of 1024-QAM for PDSCH is signalled for the band. Value f0p4 indicates the scaling factor 0.4, f0p75 indicates 0.75, and so on. If absent, the scaling factor 1 is applied to the band in the max data rate calculation.UE indicating support of this feature shall also indicate support of *pdsch-1024QAM-FR1-r17* or *pdsch-1024QAM-2MIMO-FR1-r17* to the band. | FS | No | N/A | FR1 only |
| ***scellWithoutSSB***Defines whether the UE supports configuration of SCell that does not transmit SS/PBCH block. This is conditionally mandatory with capability signalling for intra-band CA but not supported for inter-band CA. | FS | CY | N/A | N/A |
| ***searchSpaceSharingCA-DL***Defines whether the UE supports DL PDCCH search space sharing for carrier aggregation operation. | FS | No | N/A | N/A |
| ***sfn-SchemeA-r17***Indicates whether the UE supports SFN scheme A for PDCCH scheduling SFN Scheme A PDSCH. | FS | No | N/A | N/A |
| ***sfn-SchemeA-DynamicSwitching-r17***Indicates whether the UE supports dynamic switching between single-TRP and PDSCH SFN scheme A by TCI state field in DCI formats 1\_1 and 1\_2. The UE supporting this feature shall indicate *sfn-SchemeA-r17* or *sfn-SchemeA-PDSCH-only-r17*. | FS | No | N/A | N/A |
| ***sfn-SchemeA-PDCCH-only-r17***Indicates whether the UE supports SFN scheme A for PDCCH scheduling single TRP for PDSCH. | FS | No | N/A | N/A |
| ***sfn-SchemeA-PDSCH-only-r17***Indicates whether the UE supports SFN scheme A for PDSCH scheduled by single TRP PDCCH. | FS | No | N/A | N/A |
| ***sfn-SchemeB-r17***Indicates whether the UE supports SFN scheme B for PDCCH scheduling SFN Scheme B PDSCH. | FS | No | N/A | N/A |
| ***sfn-SchemeB-DynamicSwitching-r17***Indicates whether the UE supports dynamic switching between single-TRP and PDSCH SFN scheme B by TCI state field in DCI formats 1\_1 and 1\_2.The UE supporting this feature shall indicate *sfn-schemeB-r17* or *sfn-schemeB-PDSCH-only-r17.* | FS | No | N/A | N/A |
| ***sfn-SchemeB-PDSCH-only-r17***Indicates whether the UE supports SFN scheme B for PDSCH scheduled by single TRP PDCCH. | FS | No | N/A | N/A |
| ***singleDCI-SDM-scheme-r16***Indicates whether the UE supports single DCI based spatial division multiplexing scheme. | FS | No | N/A | N/A |
| ***sps-Multicast-r17***Indicates whether the UE supports SPS group-common PDSCH for multicast on PCell, comprised of the following functional components:- Supports one SPS group-common PDSCH configuration for multicast;- Supports {2, 4, 8} times semi-static slot-level repetition for SPS group-common PDSCH.A UE supporting this feature shall also indicate support of *dynamicMulticastPCell-r17*. | FS | No | N/A | N/A |
| ***supportedSRS-Resources***Defines support of SRS resources for SRS carrier switching for a band without associated FeatureSetuplink. The capability signalling comprising indication of:- *maxNumberAperiodicSRS-PerBWP* indicates supported maximum number of aperiodic SRS resources that can be configured for the UE per each BWP- *maxNumberAperiodicSRS-PerBWP-PerSlot* indicates supported maximum number of aperiodic SRS resources per slot in the BWP- *maxNumberPeriodicSRS-PerBWP* indicates supported maximum number of periodic SRS resources per BWP- *maxNumberPeriodicSRS-PerBWP-PerSlot* indicates supported maximum number of periodic SRS resources per slot in the BWP- *maxNumberSemiPersistentSRS-PerBWP* indicate supported maximum number of semi-persistent SRS resources that can be configured for the UE per each BWP- *maxNumberSemiPersistentSRS-PerBWP-PerSlot* indicates supported maximum number of semi-persistent SRS resources per slot in the BWP- *maxNumberSRS-Ports-PerResource* indicates supported maximum number of SRS antenna port per each SRS resourceIf the UE indicates the support of srs-CarrierSwitch for this band and this field is absent, the UE supports one periodic, one aperiodic, no semi-persistent SRS resources per BWP per slot and one SRS antenna port per SRS resource. | FS | FD | N/A | N/A |
| ***timeDurationForQCL, timeDurationForQCL-v1710***Defines minimum number of OFDM symbols required by the UE to perform PDCCH reception and applying spatial QCL information received in DCI for PDSCH processing as described in TS 38.214 [12] clause 5.1.5. The number of OFDM symbols is measured from the end of the last symbol of the PDCCH reception to the start of the first symbol of the PDSCH reception. UE shall indicate one value of the minimum number of OFDM symbols per each subcarrier spacing of 60kHz, 120kHz, 480kHz and 960kHz. | FS | Yes | N/A | FR2 only |
| ***twoFL-DMRS-TwoAdditionalDMRS-DL***Defines whether the UE supports DM-RS pattern for DL transmission with 2 symbols front-loaded DM-RS with one additional 2 symbols DM-RS. | FS | No | N/A | N/A |
| ***type1-3-CSS***Defines whether the UE is able to receive PDCCH in FR2 in a Type1-PDCCH common search space configured by dedicated RRC signalling, in a Type3-PDCCH common search space or a UE-specific search space if those are associated with a CORESET with a duration of 3 symbols. | FS | Yes | N/A | FR2 only |
| ***ue-SpecificUL-DL-Assignment***Indicates whether the UE supports dynamic determination of UL and DL link direction and slot format based on Layer 1 scheduling DCI and higher layer configured parameter *TDD-UL-DL-ConfigDedicated* as specified in TS 38.213 [11]. | FS | No | N/A | N/A |

#### 4.2.7.6 *FeatureSetDownlinkPerCC* parameters

| **Definitions for parameters** | **Per** | **M** | **FDD-TDD****DIFF** | **FR1-FR2****DIFF** |
| --- | --- | --- | --- | --- |
| ***broadcastSCell-r17***Indicates whether the UE supports MBS reception via broadcast in RRC\_CONNECTED, on one frequency indicated in an *MBSInterestIndication* message, when an SCell is configured and activated on that frequency, as specified in TS 38.331 [9].NOTE: The UE is not required to receive MBS via broadcast on PCell and SCell simultaneously | FSPC | No | No | No |
| ***channelBW-90mhz***Indicates whether the UE supports the channel bandwidth of 90 MHz.For FR1, the UE shall indicate support according to TS 38.101-1 [2], Table 5.3.5-1. | FSPC | CY | N/A | FR1 only |
| ***dci-BroadcastWith16Repetitions-r17***Indicates whether the UE supports up to 16 times dynamic slot-level repetition for broadcast MTCH. | FSPC | No | No | No |
| ***fdm-BroadcastUnicast-r17***Indicates whether the UE supports overlapping PDSCH reception that one unicast PDSCH and one group-common PDSCH for broadcast in RRC CONNECTED in a slot are partially or fully overlapping in time domain and non-overlapping in frequency domain.A UE supporting this feature shall also support broadcast reception as specified in clause 5.10. | FSPC | No | N/A | N/A |
| ***fdm-MulticastUnicast-r17***Indicates whether the UE supports overlapping PDSCH reception that one unicast PDSCH and one group-common PDSCH for multicast in RRC CONNECTED in a slot are partially or fully overlapping in time domain and non-overlapping in frequency domain.A UE supporting this feature shall also indicate support of *dynamicMulticastPCell-r17.*NOTE: The UE supporting this feature is not required to support FDMed SPS. | FSPC | No | N/A | N/A |
| ***intraSlotTDM-UnicastGroupCommonPDSCH-r17***Indicates whether the UE supports Intra-slot TDM-ed unicast PDSCH and group-common PDSCH. The value indicates that for any two consecutive slots n and n+1, if there are more than 1 broadcast/multicast/unicast PDSCH in either slot, whether to require the minimum time separation (4 OFDM symbols for 30kHz and 7 OFDM symbols for 60kHz) between starting time of any two broadcast/multicast/unicast PDSCHs within the duration of these slots.This feature includes the following functional components:- Supports TDM between one unicast PDSCH and one group-common PDSCH in a slot;- Support TDM between M (M>1) TDMed unicast PDSCHs and one group-common PDSCH in a slot per CC;- Support TDM among N (N>1) group-common PDSCHs in a slot per CC;- Support TDM between K (K>1) TDMed unicast PDSCHs and L (L>1) TDMed group-common PDSCHs in a slot per CC;- The UE maximum number of TDMed PDSCH receptions capability in a slot per CC is kept based on *pdsch-ProcessingType1-DifferentTB-PerSlot*;- Up to one broadcast PDSCH is supported in a slot.A UE supporting this feature shall support broadcast reception as specified in clause 5.10 and/or indicate support of *dynamicMulticastPCell-r17*, and shall indicate support of *pdsch-ProcessingType1-DifferentTB-PerSlot*.NOTE1: Group-common PDSCH(s) are counted as unicast PDSCH(s).NOTE2: The max number of (M+1), N, (K+L) are determined based on the numbers reported by *pdsch-ProcessingType1-DifferentTB-PerSlot*. | FSPC | No | N/A | N/A |
| ***supportedCRS-InterfMitigation-r17***Indicates whether the UE supports CRS interference mitigation (CRS-IM) in both DSS and non-DSS scenarios with overlapping spectrum for LTE and NR, which is defined in TS 38.101-4 [18]. The capability signalling contains the following:- *crs-IM-DSS-15kHzSCS-r17* indicates whether the UE supports neighboring LTE cell CRS-IM in DSS scenario with NR 15 kHz SCS. UE can indicate support of this capability on the CC(s) in a band only if the UE indicates support of *rateMatchingLTE-CRS* on that band.- *crs-IM-nonDSS-15kHzSCS-r17* indicates whether the UE supports neighboring LTE cell CRS-IM in non-DSS and 15 kHz NR SCS scenario, without the assistance of network signalling on LTE channel bandwidth.- *crs-IM-nonDSS-NWA-15kHzSCS-r17* indicates whether the UE supports neighboring LTE cell CRS-IM in non-DSS and 15 kHz NR SCS scenario, with the assistance of network signalling on LTE channel bandwidth.- *crs-IM-nonDSS-30kHzSCS-r17* indicates whether the UE supports neighboring LTE cell CRS-IM in non-DSS and 30 kHz NR SCS scenario, without the assistance of network signalling on LTE channel bandwidth.- crs*-IM-nonDSS-NWA-30kHzSCS-r17* indicates whether the UE supports neighboring LTE cell CRS-IM in non-DSS and 30 kHz NR SCS scenario, with the assistance of network signalling on LTE channel bandwidth.For the UE supporting the capability of *crs-IM-DSS-15kHzSCS-r17*, the UE can perform CRS-IM without the assistant configuration information of neighbour LTE cells when *RateMatchPatternLTE-CRS* is configured for the serving cell, and if *lte-NeighCellsCRS-Assumptions-r17* is not configured.For the UE supporting the capability of *crs-IM-nonDSS-15kHzSCS-r17*, the UE can perform CRS-IM without the assistant configuration information of neighbour LTE cells with 15 kHz SCS when *RateMatchPatternLTE-CRS* is not configured for the serving cell, and if *MeasObjectEUTRA* is configured, the configured measurement gaps overlap with neighbour LTE cell PBCH position and *lte-NeighCellsCRS-Assumptions-r17* is not configured*.*For the UE supporting the capabilities of *crs-IM-nonDSS-30kHzSCS-r17*, the UE can perform CRS-IM without the assistant configuration information of neighbour LTE cells with 30 kHz SCS when *RateMatchPatternLTE-CRS* is not configured for the serving cell, and if *MeasObjectEUTRA* is configured, the configured measurement gaps overlap with neighbour LTE cell PBCH position and *lte-NeighCellsCRS-Assumptions-r17* is not configured.NOTE 1: In the DSS scenario, serving and neighboring cells are both operating with dynamic spectrum sharing (DSS) of NR and LTE.NOTE 2: In the non-DSS scenario, serving cell is operating in NR, and neighboring cells are operating in LTE. | FSPC | No | No | FR1 only |
| ***dynamicMulticastSCell-r17***Indicates whether the UE supports to receive group-common PDCCH/PDSCH with CRC scrambled by G-RNTI for SCell on one frequency, when an SCell is configured and activated on that frequency, as specified in TS 38.331 [9].A UE supporting this feature shall also indicate support of *dynamicMulticastPCell-r17*.NOTE: UE is not expected to be configured simultaneously with more than one component carrier for multicast reception. | FSPC | No | N/A | N/A |
| ***maxModulationOrderForMulticastDataRateCalculation-r17***Defines the maximum modulation order used for maximum data rate calculation for multicast PDSCH.- For FR1, up to 1024QAM is supported as maximum modulation order used for maximum data rate calculation for multicast PDSCH, with candidate values {qam256, qam1024}.- For FR2, up to 256QAM is supported as maximum modulation order used for maximum data rate calculation for multicast PDSCH, with candidate values {qam64, qam256}.A UE supporting this feature shall also indicate support of *dynamicMulticastPCell-r17*. | FSPC | No | N/A | N/A |
| ***maxNumberMIMO-LayersPDSCH***Defines the maximum number of spatial multiplexing layer(s) supported by the UE for DL reception. For single CC standalone NR, it is mandatory with capability signalling to support at least 4 MIMO layers in the bands where 4Rx is specified as mandatory for the given UE and at least 2 MIMO layers in FR2. If absent, the UE does not support MIMO on this carrier.For the bands where *DL-1024QAM-2MIMO-FR1-r17* is indicated, MIMO layers for 1024 QAM is the smaller value between 2 and *maxNumberMIMO-LayersPDSCH.* i.e. *maxNumberMIMO-LayersPDSCH* applies for the modulation orders other than 1024 QAM. | FSPC | CY | N/A | N/A |
| ***maxNumberMIMO-LayersMulticastPDSCH-r17***Defines the maximum number of spatial multiplexing layer(s) supported by the UE for multicast PDSCH. If not reported, UE supports 1 MIMO layer only for multicast PDSCH.A UE supporting this feature shall also indicate support of *dynamicMulticastPCell-r17*.NOTE: If the UE supports up to 8 layers, the UE supports second TB (TB2). | FSPC | No | N/A | N/A |
| ***multiDCI-MultiTRP-r16***Indicates whether the UE supports multi-DCI based multi-TRP PDSCH/PUSCH operation and support of fully/partially overlapping PDSCHs in time and non-overlapping in frequency. This capability applies only to BWPs where two values of *coresetPoolIndex* are configured. The capability signalling contains the following:- *maxNumberCORESET-r16* indicates maximum number of CORESETs configured per BWP per cell in addition to CORESET 0 for multi-DCI based multi-TRP PDSCH/PUSCH operation.- *maxNumberCORESETPerPoolIndex-r16* indicates maximum number of CORESETs configured per *coresetPoolIndex* per BWP per cell in addition to CORESET 0 for multi-DCI based multi-TRP PDSCH/PUSCH operation.- *maxNumberUnicastPDSCH-PerPool-r16* indicates maximum number of unicast PDSCHs per *coresetPoolIndex* per slot.NOTE 1: A UE may assume that its maximum receive timing difference between the DL transmissions from two TRPs is within a Cyclic Prefix.NOTE 2: Processing capability 2 is not supported in any CC if at least one CC is configured with two values of *coresetPoolIndex*.NOTE 3: If UE reports value N1 for *maxNumberCORESET-r16*, that means UE supports up to min (N1+1, 5) CORESETs in total (including CORESET#0) if there is CORESET#0, and supports maximal N1 CORESETs if there is no CORESET#0.NOTE 4: If UE reports value N2 for *maxNumberCORESETPerPoolIndex-r16*, that means UE supports up to min (N2+1, 3) CORESETs in total (including CORESET#0) for a TRP if there is CORESET#0, and supports maximal N2 CORESETs for another TRP if there is no CORESET#0.NOTE 5: For the multi-DCI based multi-TRP PUSCH operation, the maximum number of unicast PUSCHs that UE can support per slot is based on *pusch-ProcessingType1-DifferentTB-PerSlot*, and it is counted across both *coresetPoolIndex* of TRPs. | FSPC | No | N/A | N/A |
| ***sps-MulticastSCell-r17***Indicates whether the UE supports one SPS group-common PDSCH configuration for multicast for SCell, comprised of the following functional components:- Supports one SPS group-common PDSCH configuration for multicast for SCell;- Supports {2, 4, 8} times semi-static slot-level repetition for SPS group-common PDSCH for SCell.A UE supporting this feature shall also indicate support of *sps-Multicast-r17* and *dynamicMulticastSCell-r17*. | FSPC | No | N/A | N/A |
| ***sps-MulticastSCellMultiConfig-r17***Indicates whether the UE supports up to 8 SPS group-common PDSCH configurations per CFR for multicast for SCell. The value indicates the maximum number of activated SPS group-common PDSCH configurations per CFR for multicast for SCell.The total number of SPS configurations for both multicast and unicast is no larger than 8 in a BWP of a serving cell. The total number of SPS configurations for both multicast and unicast in a cell group is no larger than 32.A UE supporting this feature shall also indicate support of *sps-MulticastSCell-r17*. | FSPC | No | N/A | N/A |
| ***supportedBandwidthDL, supportedBandwidthDL-v1710***Indicates maximum DL channel bandwidth supported for a given SCS that UE supports within a single CC (and in case of DAPS handover for the source or target cell), which is defined in Table 5.3.5-1 in TS 38.101-1 [2] for FR1 and Table 5.3.5-1 in TS 38.101-2 [3] for FR2.For FR1, all the bandwidths listed in TS38.101-1 Table 5.3.5-1 for each band shall be mandatory with a single CC unless indicated optional. For FR2, the set of mandatory CBW is 50, 100, 200 MHz. When this field is included in a band combination with a single band entry and a single CC entry (i.e. non-CA band combination), the UE shall indicate the maximum channel bandwidth for the band according to TS 38.101-1 [2] and TS 38.101-2 [3]. *supportedBandwidthDL-v1710* is included if the maximum DL channel bandwidth supported by the UE within a single CC is greater than 400MHz, otherwise it is absent.The UE may report a *supportedBandwidthDL* wider than the *channelBWs-DL*; this *supportedBandwidthDL* may not be included in the Table 5.3.5-1 of TS 38.101-1[2]/TS 38.101-2[3] for the case that the UE is unable to report the actual supported bandwidth according to the Table 5.3.5-1 of TS 38.101-1[2]/TS 38.101-2[3]. For each band, RedCap UEs shall indicate its maximum channel bandwidth, which is the maximum of those channel bandwidths that are less than or equal to 20 MHz for FR1 and less than or equal to 100 Mhz for FR2, taking restrictions in TS 38.101-1 [2] and TS 38.101-2 [3] into consideration.NOTE: To determine whether the UE supports a channel bandwidth of 90 MHz, the network may ignore this capability and validate instead the *channelBW-90mhz*, the *supportedBandwidthCombinationSet* and the *supportedBandwidthCombinationSetIntraENDC*. To determine whether the UE supports a channel bandwidth of 400 MHz, the network validates this capability, the *supportedBandwidthCombinationSet*, and the *supportedBandwidthCombinationSetIntraENDC*. For serving cell(s) with other channel bandwidths the network validates the *channelBWs-DL*, the *supportedBandwidthCombinationSet*, the *supportedBandwidthCombinationSetIntraENDC*, the *asymmetricBandwidthCombinationSet* (for a band supporting asymmetric channel bandwidth as defined in clause 5.3.6 of TS 38.101-1 [2]), *supportedBandwidthDL/supportedBandwidthDL-v1710* and *supportedMinBandwidthDL*. | FSPC | CY | N/A | N/A |
| ***supportedMinBandwidthDL-r17***Indicates minimum DL channel bandwidth supported for a given SCS that UE supports within a single CC (and in case of intra-frequency DAPS handover for the source and target cells), which is defined in Table 5.3.5-1 in TS 38.101-1 [2] for FR1 and Table 5.3.5-1 in TS 38.101-2 [3] for FR2. This parameter is only applicable to the Bandwidth Combination Set 5. This field does not restrict the bandwidths configured for a single CC (i.e. non-CA case). | FSPC | CY | N/A | N/A |
| ***supportedModulationOrderDL***Indicates the maximum supported modulation order to be applied for downlink in the carrier in the max data rate calculation as defined in 4.1.2. If included, the network may use a modulation order on this serving cell which is higher than the value indicated in this field as long as UE supports the modulation of higher value for downlink. If not included:- for FR1, the network uses the modulation order signalled per band i.e. *pdsch-1024QAM-FR1-r17* or *pdsch-1024QAM-2MIMO-FR1-r17* when *pdsch-1024QAM-FR1-r17* or *pdsch-1024QAM-2MIMO-FR1-r17* is signalled for the band, otherwise the network uses the modulation order signalled in *pdsch-256QAM-FR1*.- for FR2, the network uses the modulation order signalled per band i.e. *pdsch-256QAM-FR2* if signalled. If not signalled in a given band, the network shall use the modulation order 64QAM.In all the cases, it shall be ensured that the data rate does not exceed the max data rate (*DataRate*) and max data rate per CC (*DataRateCC*) according to TS 38.214 [12]. | FSPC | No | N/A | N/A |
| ***supportedSubCarrierSpacingDL***Defines the supported sub-carrier spacing for DL by the UE, as defined in clause 4.2-1 of TS 38.211 [6], indicating the UE supports simultaneous reception with same or different numerologies in CA. Support of simultaneous reception with same numerology for intra-band NR CA including both contiguous and non-contiguous is mandatory with capability in both FR1 and FR2. Support of simultaneous reception with two different numerologies between FR1 band(s) and FR2 band(s) in DL is mandatory with capability if UE supports inter-band NR CA including both FR1 band(s) and FR2 band(s). Optional for other cases. Support of simultaneous reception of with different numerologies in CA for other cases is optional. | FSPC | CY | N/A | N/A |
| ***supportFDM-SchemeB-r16***Indicates whether UE supports single DCI based FDMSchemeB. | FSPC | No | N/A | N/A |

|  |
| --- |
| END OF CHANGE |