|  |  |  |  |
| --- | --- | --- | --- |
| Company | Clause | Comment | Rapp Response |
| OPPO | 16.9.x.2 | **This** should be applicable to all cases, rather than limited to “default SLRB is used for a QoS flow and the SL-CAPC of the default SLRB is not configured”When the default SLRB is used for the QoS flow and the SL-CAPC of the default SLRB is not configured, the UE derives SL-CAPC directly from the table below for standardized PQI and **selects the lowest SL-CAPC priority level (highest SL-CAPC value) among the associated QoS flows**.  |  |
|  |  | **It** is not always the case, but should limited to the case where “default SLRB is used for a QoS flow and the SL-CAPC of the default SLRB is not configured”For non-standardized PQI, the UE may s**elect selects the SL-CAPC of the standardized PQI having the which best matches the QoS characteristics of the non-standardized PQI based on the closest PDB**. |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |