3GPP TSG-RAN2 Meeting #123-bis R2-231xxxx

Xiamen, China, 9~14 October 2023

Agenda Item: 7.22.3

Source: Qualcomm

Title: Summary of [Post123][060][LPWUS] Low-power receiver in RRC Connected (Qualcomm)

Document for: Discussion and Decision

# **Introduction**

This report provides a summary of the following post-meeting email discussion:

* [Post123][060][LPWUS] Low-power recevier in RRC Connected (Qualcomm)

Scope: Collect comments for and if possible progress proposals in RAN2 scope (e.g. impact to / relation to DRX, other MAC impacts). Can also collect comments for and discuss proposals for which RAN2 impact is not clear yet (e.g. not clear if MAC impact etc), up to Rapporteur what to include.

Intended outcome: Report with agreeable points, points for discussion, FFS points, pave the way for a first set of agreements etc for RRC Connected.

Deadline: Long

The deadlines for this discussion are the following:

* **September 19th 18:00 UTC:** deadline forcompanies’ feedback;
* **September 20th 18:00** **UTC**: deadline for the rapporteur to provide a summary for review;
* **September 22nd 18:00 UTC**: hard deadline for companies’ feedback on the summary.

# **Contact information**

|  |  |  |
| --- | --- | --- |
| Company | Name | Email |
| OPPO | Haitao Li | lihaitao@oppo.com |
| Nokia | Sunyoung LEE | sunyoung.lee@nokia.com |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

# **Discussion**

Per instruction by the Chair, the objective of this email discussion is to discuss possible use cases of low-power receiver in RRC Connected. The discussion points are generated based on proposals in the submitted contributions ([1]~ [13]). If possible, we will try to produce a set of proposals for discussion and agreement at the next RAN2 meeting (RAN#123bis).

As this email discussion is for the SI, the rapporteur would like to suggest that we focus our discussion only on stage-2 issues. The discussion is organized into four areas, as follows:

* Whether and how LP-WUS may be used outside DRX active time (e.g. similar to legacy wakeup signaling for DRX on duration);
* Whether and how LP-WUS may be used inside DRX active time (e.g. associated with PDCCH monitoring adaptation);
* Whether and how LP-WUS may be used for RRM measurements in RRC Connected;
* Options for de-/activating LP-WUS monitoring.

Before starting the discussion, the rapporteur would like to cite the RAN1 agreements that are related to the use of LP-WUS in RRC Connected, since they are relevant to this email discussion:

|  |
| --- |
| * + In RRC CONNECTED mode, LP-WUS monitoring can be activated/deactivated by at least one or more of     - by gNB RRC signaling, with or without UE assistance.     - by gNB L1/L2 LP-WUS activation/deactivation signaling, with or without UE assistance.     - based on pre-configured condition(s), such as timer.     - LP-WUS monitoring by UE is known to gNB, study whether it could be transparent to gNB.     - other options are not precluded. * In RRC CONNECTED mode, study benefit of LP-WUS over existing Rel-15, R16, and R17 power saving techniques for following functionalities: * LP-WUS with similar functionality as R16 DCP. * LP-WUS activates/resumes PDCCH monitoring when LP-WUS is received.   + interaction with legacy power saving techniques, if any * other functionalities are not precluded * for evaluation   + companies to report     - assumption on MR sleep state when LP-WUR is monitoring LP-WUS     - deep sleep,     - light sleep,     - micro sleep   + how to activate/deactivate LP-WUS monitoring and deactivate/activate PDCCH monitoring   + LP-WUS waveform |

## LP-WUS outside DRX active time

Many contributions have proposed that LP-WUS can be used in conjunction with DRX, e.g. LP-WUS is monitored outside DRX active time and can be used to wake up MR to start procedures related to DRX on duration timer ([1][4][5][6][7][8][9][10][11][12][13]).

However, there are different views on how exactly LP-WUS may be used in this use case. More specifically, the proposals may be classified into the following three options:

* LP-WUS replaces DCP and these two types of wakeup signals are not configured/used simultaneously ([4][5][6][10][11][12]);
* Both LP-WUS and DCP can be configured for a UE. However, UE may use only one of them at any time, e.g. depend on network configuration or link quality, etc. ([1][4][6][9]);
* LP-WUS is used in conjunction with DCP, e.g. LP-WUS first wakes up MR, which then monitors DCP ([4][6][8] [10][12]).

Next, we first discuss whether the use of LP-WUS outside DRX active time should be studied. Then for

**Q1. Which one of the following options do you support on the use of LP-WUS outside DRX active time, in which case LP-WUS wakes up MR to start procedures related to DRX timer(s)?**

1. **There is no need to study the use of LP-WUS for waking up MR to start procedures related to DRX timer(s);**
2. **LP-WUS replaces DCP and these two types of wakeup signals are configured/used simultaneously;**
3. **Both LP-WUS and DCP can be configured for a UE. However, UE may use only one of them at any time, e.g. depend on network configuration or link quality, etc.**
4. **LP-WUS is used in conjunction with DCP, e.g. LP-WUS first wakes up MR, which then monitors DCP.**
5. **LP-WUS can be used at any time to wake up MR to enter DRX Active Time to monitor PDCCH.**

You may select more than one option in your reply.

|  |  |  |
| --- | --- | --- |
| **Company** | **Option** | **Comments** |
| OPPO | Option 5 | We agree to study the use of LP-WUS for waking up MR to start procedures related to DRX timer(s), but maybe no need to restrict to drx-onDurationTimer only. Given that the power consumption of LP-WUS monitoring is ultra-low, it would be more flexible to allow LP-WUS to be used at any time to wake up MR to enter DRX Active Time to monitor PDCCH. |
| Nokia | Option 5 | Although there can be some similarities between DCP and LP-WUS, we would see they are different features and LP-WUS can be used with or without DRX, i.e., not limited to on duration. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

## LP-WUS and PDCCH monitoring adaptation

There are proposals on using LP-WUS to enhance legacy PDCCH monitoring adaptation (e.g. PDCCH skipping, SSSG switching, etc):

* In [1] [9], it is proposed that LP-WUS can be used to resume/activate PDCCH monitoring during active time;
* In [2], it is proposed that LP-WUS can be used to control PDCCH monitoring at any time;
* In [6][13], it is proposed to study the relationship between LP-WUS and legacy UE power saving techniques, e.g. C-DRX, DCP, PDCCH skipping, SSSG switching.

In legacy, PDCCH monitoring adaption has been mostly in RAN1’s domain and transparent to upper layers, with certain exceptions (e.g. UL transmissions such as SR triggers termination of PDCCH skipping). Since RAN1 has already agreed that UE can activate/resume PDCCH monitoring when LP-WUS is received and interactions with legacy power saving techniques will be studied, the rapporteur would like to suggest that we discuss this topic from RAN2’s perspective, e.g. what RAN2 impacts should be studied.

**Q2. What should RAN2 study to support the use of LP-WUS in conjunction with legacy PDCCH monitoring adaptation features (e.g. use cases listed above)?**

|  |  |
| --- | --- |
| **Company** | **Comments** (Please be specific, if possible) |
| OPPO | See our comments on Q1 |
| Nokia | At least DRX interaction should be studied. RAN2 need to discuss not only how to start PDCCH monitoring, e.g., impact on various DRX timers, but also how to switch back to LP-WUS by considering DRX timers running. |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

## Use of LP-WUS in RRM measurement

There are multiple contributions discussing the use of low-power radio/signaling in RRM measurements but with mixed views. For example,

* In [1][10], it is proposed that LP-WUR can be used for serving cell measurements or neighbor cell measurements to reduce the use of measurement gaps;
* In [2][7], it is argued that RRM measurement by MR is enough for RRC connected. Use of LP-WUR for RRM measurements is not well justified.
* In [5][8][9], it is proposed that the study for RRM measurements based on LP-WUS in RRC Connected can be postponed until its feasibility is confirmed by RAN1 and RAN4.

The rapporteur thinks that these three views cover most of the possible options and hence would like to invite your views on them. When you comment, please keep in mind that our discussion here is only from RAN2’s perspectives.

**Q3. Which of the following three views would you support?**

1. **In RRC Connected, LP-WUR can be used for serving cell measurements and/or neighbor cell measurements (additional options in Q5);**
2. **Use of LP-WUR for RRM measurements in RRC connected is not studied.**
3. **The study for use of LP-WUR for RRM measurements in RRC Connected can be postponed until its feasibility is confirmed by RAN1 and RAN4.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Option** | **Comments** (Please provide reasons if possible) |
| OPPO | Option 3 | RRM measurements in RRC Connected was discussed in RAN1 with the following agreements made in RAN1#112bis-e.   |  | | --- | | Agreement   * For RRC connected mode, the following is assumed for LP-WUS study in RAN1   + RLM/BFD/CSI are performed by UE Main Radio (MR)   + RRM measurements are performed by UE Main Radio (MR)   + Ultra-deep sleep state is not allowed for MR.   Study additional support of RRM measurement by LP-WUR for RRC connected mode |   Since the feasibility of RRM measurements by LP-WUS in RRC Connected will need further study in RAN1, RAN2 can postpone the discussion on this topic. |
| Nokia | Option 3 | Although we see that RRC measurement in RRC\_CONNECTED is one area that RAN2 need to study, more time seems to be needed for RAN1. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Q4. If you selected Option 1 in Q4, please indicate which one of the following options you support:**

1. **LP-WUR is used only for serving cell RRM measurements;**
2. **LP-WUR is used only for neighbor cell RRM measurements;**
3. **LP-WUR can be used for any type of RRM measurements.**

You may select more than one option. All options are for RRC Connected.

Again, our discussion here is only from RAN2’s perspective, if RAN1/4 can confirm their feasibility.

|  |  |  |
| --- | --- | --- |
| **Company** | **Option** | **Comments** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

## De-/activation of LP-WUS

There are a number of contributions discussing conditions for de-/activating LP-WUS monitoring ([1][4][5][6][13]). Since the proposals are rather diverse, the rapporteur summarize them as follows:

* Monitoring of LP-WUS is de-/activated based on NW indication;
* Network pre-configures UE with criteria for monitoring LP-WUR. UE then autonomously de-/activate its monitoring based on its evaluation whether the configured criteria is met.
* UL/DL transmissions by MR can be an additional criterion for UE to de-activate its monitoring.

These options are consistent with what RAN1 has agreed, except the one with UL transmission. Instead of repeating what RAN1 has agreed, the rapporteur thinks that we can discuss the delta, i.e. the proposal on UL transmission deactivating LP-WUS monitoring and if any additional options should be supported.

**Q5. In addition to the options agreed by RAN1 for de-/activating LP-WUS monitoring, do you think UL transmission by MR can also be a criterion for UE to de-activate its monitoring?**

**You may also propose in the Comments column any additional options that you think should be studied.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments** |
| OPPO | Yes | UL traffic arrival should be another condition for deactivation of LP-WUS monitoring, which is triggered at UE side. |
| Nokia | Yes | Traffic can be one criterion to activate/deactivate the LP-WUS, and we should consider both UL and DL because PDCCH monitoring is for scheduling of either UL or DL. The question would be how the UE assumes that DL scheduling is less/more expected so that LP-WUS is activated/deactivated accordingly. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

## Other issues

Please comment in the table below if you think there are other issues that should be studied but have been missed in the questions above.

|  |  |
| --- | --- |
| **Company** | **Issues** (Please be specific, if possible) |
| Nokia | Given that LP-WUS monitoring is deactivated/stopped for immediate scheduling via PDCCH, RAN2 would need to study how the UE can maintain its UL synchronization during LP-WUS monitoring. If the UE is not in UL synchronized state after switching back to PDCCH monitoring, the UE cannot perform immediate data transmission and would need to perform RA procedure. We think periodic CSI report during LP-WUS monitoring would be heavy because there is no scheduling while monitoring LP-WUS and more sporadic CSI report would be sufficient.  **Proposal: RAN2 discuss how to maintain the UL synchronization while the UE monitors the LP-WUS.** |
| Nokia | We wonder what the RAN2 assumption would be for SPS and CG while the UE monitors LP-WUS and MR is in sleep, i.e., whether they are kept activated or assumed to be deactivated.  **Proposal: RAN2 discuss the LP-WUS impact on SPS and CG.** |
|  |  |

# **Conclusions**

(To be added later)

# References

1. R2-2204523, Use of low-power receiver in RRC Connected, Qualcomm Incorporated.
2. R2-2307308, Discussion on LP-WUS/WUR in RRC\_Connected, vivo.
3. R2-2307260, Discussion on LP-WUR’s operation, OPPO.
4. R2-2307345, Discussing on LP-WUS monitoring for RRC\_Connected, Xiaomi Communications.
5. R2-2307424, Discussion on LP-WUS in RRC\_CONNECTED state, CATT.
6. R2-2307449, High layer procedures for LP-WUS in RRC\_CONNECTED state, Huawei, HiSilicon.
7. R2-2307462, Discussion on the considerations for LPWUS in RRC\_CONNECTED, NEC Corporation.
8. R2-2307592, RAN2 impacts of LP-WUS in connected mode ZTE Corporation, Sanechips.
9. R2-2307849, RAN2 impact of LP-WUS in RRC\_CONNECTED state, Apple.
10. R2-2308461, LP-WUS in RRC Connected Mode, Lenovo.
11. R2-2308532, Discussion on LP-WUS in RRC\_CONNECTED, Continental Automotive .
12. R2-2308810, LP-WUS/WUR for RRC Connected, Ericsson.
13. R2-2308748, On LP-WUS in RRC\_CONNECTED Nokia, Nokia Shanghai Bell