|  |  |  |  |
| --- | --- | --- | --- |
| Company | Clause | Comment | Rapp Response |
| Apple | 16.9.Y | Issue:" Carrier (re)selection may be performed and a new carrier configuration is reported to the RX UE when the TX UE detects carrier failure on a specific carrier, as specified in 3GPP TS 38.321 [x]."It is not clear what "a new carrier configuration is reported to the RX UE" means, and we generally don't say a configured is reported. Solution:According to below agreement in last RAN2 meeting:**Agreements on SL RLF**1. In TX UE, per carrier “carrier failure” is introduced. If “carrier failure” is declared for a carrier, the carrier should be removed/released. The carrier (re)selection can be triggered. For UC, this carrier can be released via PC5 RRC reconfiguration.

We suggest below change: " When the TX UE detects carrier failure on a specific carrier, carrier (re)selection may be performed and the concerned carrier can be released via PC5 RRC reconfiguration, as specified in 3GPP TS 38.321 [x]."[OPPO] Same view here |  |
| Huawei, HiSilicon | 16.9.Y | Not clear this sentence "Carrier selection and logical channel prioritization is performed similar to groupcasat and broadcast among the carriers delivered in the carrier configuration" is for UC only or applies to all cast types. If for all cast types, can remove "similiar to groupcast and broadcast". If it is for UC, shall keep "For unicast", or merge this sentence with the previous sentence.  |  |
| OPPO | 16.9.Y | Also for this sentenceCarrier selection and logical channel prioritization is performed similar to groupcasat and broadcast among the carriers delivered in the carrier configurationWhen combine LCP and the last part together, the meaning is unclear, it seems to say the LCP would be based on the carrier configured, but in fact LCP has to taken a lot of aspect into account (e.g., even the flow2carrier mapping thing is not so clear yet), how about remove the LCP part and leave it to stage-3? |  |
| Xiaomi | 16.9.x.4 | and the responding UE can utilize a COT shared by a COT initiating UE based on matching the responding UE’s source/destination with the additional ID(s).suggest to revise to and the responding UE can utilize a COT shared by a COT initiating UE if the destination/source ID of the responding UE’s transmission match the source/destination indicated by the additional ID(s)Also wonder if need to have separate description for unicast and BC/GC for additional IDs.  |  |
| Xiaomi | 16.9.x.4 | In groupcast/broadcast, the responding UE’s destination ID should match the initiator’s destination ID.To align with unicast, suggest to change to “In groupcast/broadcast, the destination ID of the responding UE’s transmission should match the destination ID of the initiator UE’s transmission.” |  |
| Xiaomi | 16.9.Y | It is not clear what “carrier failure” refers to, suggest to add for which the HARQ based DTX counting reaching the maximum as specified in 3GPP TS 38.321 [x] |  |
| Xiaomi | 16.9.Y | For a SL DRB, sidelink packet duplication is (pre)configured in the bearer configuration. The above sentence imply UE follows NW configuration to enable/disable PDCP duplication? Actually according to the agreement, for some cases, it is up to UE implementation. TX UE configures PDCP duplication to the RX UE for SRB and DRB should be captured in general.Also how to select carrier set should be more or less reflected?  |  |