3GPP TSG-RAN WG2 Meeting #123bis R2-230xxxx

Xiamen, China, 9-13 October 2023

**Agenda item: 6.4.1**

**Source: CATT**

**Title:** **[Post123bis][402][POS] BDS B1C corrections (CATT)**

**WID/SID: NR\_pos\_enh2-Core**

**Document for: Discussion and Agreement**

# 1 Introduction

This document is to kick off the following email discussion:

* [Post123bis][402][POS] BDS B1C corrections (CATT)

      Scope: Discuss the proposal in R2-2311372 and develop a CR for next meeting, considering also the broadcast case.

      Intended outcome: Agreeable CR

      Deadline: Long

In this email discussion the following contribution related with BDS B1C corrections, i.e., including correction of existing SSR IEs for BDS B1C signal to decide if these contributions or proposals in the contributions can be agreed.

1. [R2-2311372](https://www.3gpp.org/ftp/Meetings_3GPP_SYNC/RAN2/Inbox/R2-2311372.zip) Report of [AT123bis][415][POS] BDS B1C corrections (CATT) CATT discussion Rel-17
2. [R2-2311572](file:///C%3A%5CUsers%5Cmtk16923%5CDocuments%5C3GPP%20Meetings%5C202310%20-%20RAN2_123bis%2C%20Xiamen%5CExtracts%5CR2-2311572_37355_CR0466r2_%28Rel-17%29.docx) Correction of existing SSR IEs in A-GNSS for BDS system CATT, CAICT, CMCC, China Telecom, China Unicom, Huawei, ZTE Corporation, MediaTek Inc., OPPO, xiaomi, vivo, Spreadtrum CR Rel-17 37.355 17.6.0 0466 2 F NR\_pos\_enh-Core

# 2 Contact Information

Respondents to the email discussion are kindly asked to fill in the following table.

|  |  |
| --- | --- |
| Company | Contact: Name (E-mail) |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

# 3 Discussion

[R2-2311372](https://www.3gpp.org/ftp/Meetings_3GPP_SYNC/RAN2/Inbox/R2-2311372.zip) Report of [AT123bis][415][POS] BDS B1C corrections (CATT) has discussion and reach the agreeable way forward:

Introduce a new field to distinguish the reference signal for all potential GNSS and a UE capability to solve the backward compatibility in unicast LPP.

Companies will further discuss how to solve the backward compatibility in broadcast for the next meeting.

1. Proposal 1: Agree the revised CR in R2-2311572.
2. Proposal 2: Further discuss how to solve the backward compatibility in broadcast.

## 3.1 Impacts of correction for BDS B1C signal in TS 37.355

[R2-2311572](file:///C%3A%5CUsers%5Cmtk16923%5CDocuments%5C3GPP%20Meetings%5C202310%20-%20RAN2_123bis%2C%20Xiamen%5CExtracts%5CR2-2311572_37355_CR0466r2_%28Rel-17%29.docx) proposed the following correction to enable the SSR service applie to B1C-only devices in unicast:

### 3.1.1 correction #1

2 References: ICD specification of BDS PPP-B2b is added in section 2 as reference for B1C.

[XX] BDS-SIS-ICD-PPP-B2b-1.0: "BeiDou Navigation Satellite System Signal In Space Interface Control Document Precise Point Positioning Service Signal PPP-B2b (Version 1.0)", July, 2020.

### 3.1.2 correction #2

GNSS-SSR-OrbitCorrections

1. A new field *refEmph* for identifying the reference signal of B1C is included in *GNSS-SSR-OrbitCorrections* which also allows future extension.

2. The condition of the new field is added.

3. The field description of the new field is added to clarify which signal is the reference signal that the iod field refers.

4. Note 4 is added to clarify when that gnss-ID indicates 'bds' and if *refEmph* is present, the iod refers to the indicated broadcast ephemeris.

SSR-OrbitCorrectionSatelliteElement-r15 ::= SEQUENCE {

 svID-r15 SV-ID,

 iod-r15 BIT STRING (SIZE(11)),

 delta-radial-r15 INTEGER (-2097152..2097151),

 delta-AlongTrack-r15 INTEGER (-524288..524287),

 delta-CrossTrack-r15 INTEGER (-524288..524287),

 dot-delta-radial-r15 INTEGER (-1048576..1048575) OPTIONAL, -- Need ON

 dot-delta-AlongTrack-r15 INTEGER (-262144..262143) OPTIONAL, -- Need ON

 dot-delta-CrossTrack-r15 INTEGER (-262144..262143) OPTIONAL, -- Need ON

 ...,

 [[

 ssr-IntegrityOrbitBounds-r17 SSR-IntegrityOrbitBounds-r17 OPTIONAL -- Cond Integrity1

 ]],

 [[

 refEmph-r17 ENUMERATED { b1c, ... } OPTIONAL -- Cond REF

 ]]

}

| Conditional presence | Explanation |
| --- | --- |
| *Integrity1* | The field is mandatory present if *ORBIT-IntegrityParameters* is present*;* otherwise it is not present. |
| *Integrity2* | The field is mandatory present if *orbitRangeErrorCorrelationTime* is present*;* otherwise it is not present. |
| *REF* | The field is optionally present, Need ON, for none default reference signal (e.g. B1C in [XX]); otherwise it is not present. |

|  |
| --- |
| ***GNSS-SSR-OrbitCorrections field descriptions*** |
| ***iod***This field specifies the IOD value of the broadcast ephemeris for which the orbit corrections are valid (see IE *GNSS‑NavigationModel*). NOTE 2, NOTE4. |
| ***refEmph*** This field specifies which signal is the reference signal that the iod field refers to (see the IE *GNSS‑NavigationModel*) if present. |

NOTE 1: The update intervals are aligned to the GPS time scale for all GNSSs in order to allow synchronous operation for multiple GNSS services. This means that the update intervals may not be aligned to the beginning of the day for another GNSS. Due to the leap seconds, this is generally the case for GLONASS.

NOTE 2: In the cases that *gnss-ID* indicates 'gps', 'qzss' or 'bds', the *iod* refers to the NAV broadcast ephemeris (GPS L1 C/A, QZSS QZS-L1 or BDS B1I/B3I, respectively, in table GNSS to iod Bit String(11) relation in IE *GNSS‑NavigationModel*).

NOTE 3: The reference time *t0* is *epochTime* + ½ × *ssrUpdateInterval*. The reference time *t0* for *ssrUpdateInterval* '0' is *epochTime*.

NOTE 4: In the cases that *gnss-ID* indicates 'bds' and if *refEmph* is present, the *iod* refers to the indicated broadcast ephemeris (e.g. *b1c* for B-CNAV1 broadcast ephemeris (BDS B1C/B2a in table GNSS to iod Bit String(11) relation in IE *GNSS‑NavigationModel*).

### 3.1.3 correction #3

GNSS-SSR-OrbitCorrectionsSupport (Capability):

The capability to support reference signal of B1C or not is included in *GNSS-SSR-OrbitCorrectionsSupport*

#### – *GNSS-SSR-OrbitCorrectionsSupport*

-- ASN1START

GNSS-SSR-OrbitCorrectionsSupport-r15 ::= SEQUENCE {

 ...,

 [[

 orbit-IntegritySup-r17 BIT STRING { correlationTimeSup (0)

 } (SIZE(1..8)) OPTIONAL

 ]],

 [[

 bds-B1C-SSR-OrbitCorrectionsSupport-r17 ENUMERATED { supported } OPTIONAL

 ]]

}

-- ASN1STOP

| *GNSS-SSR-OrbitCorrectionsSupport* field descriptions |
| --- |
| ***orbit-IntegritySup***This field, if present, indicates that the target device supports the IEs *ORBIT-IntegrityParameters* and *SSR-IntegrityOrbitBounds*.A one‑value at the bit position '0' means that the target device supports the fields *orbitRangeErrorCorrelationTime* and *orbitRangeRateErrorCorrelationTime* in IE *ORBIT-IntegrityParameters*. |
| ***bds-B1C-SSR-OrbitCorrectionsSupport***This field, if present, indicates that the target device supports the SSR oribit correction for B1C. |

**Question 1**: Please provide comments below regarding the above corrections.

|  |  |
| --- | --- |
| Company | Comments |
|  |  |
|  |  |
|  |  |
|  |  |

## 3.2 Impacts of correction for BDS B1C signal in TS 38.331

The BDS SSR information for B1I is not the same as BDS SSR information for B1C, e.g. orbit correction. While to avoid miss-understanding, a note was introduced and clarified that B1I was the default reference signal which introduced in the last version of specification. But in some region, there are devices that only support BDS B1C, so the SSR information based on only B1C was provided. It is important to provide the high accuracy positioning service to the decives including B1I devices and single mode of B1C devices.

Considering legacy UE behaviour, a new value of GNSS ID is proposed to be added to indicate that BDS SSR information is for B1C.

###

### 6.3.1a Positioning System information blocks

– *PosSI-SchedulingInfo*

-- ASN1START

-- TAG-POSSI-SCHEDULINGINFO-START

PosSI-SchedulingInfo-r16 ::= SEQUENCE {

 posSchedulingInfoList-r16 SEQUENCE (SIZE (1..maxSI-Message)) OF PosSchedulingInfo-r16,

 posSI-RequestConfig-r16 SI-RequestConfig OPTIONAL, -- Cond MSG-1

 posSI-RequestConfigSUL-r16 SI-RequestConfig OPTIONAL, -- Cond SUL-MSG-1

 ...,

 [[

 posSI-RequestConfigRedCap-r17 SI-RequestConfig OPTIONAL -- Cond REDCAP-MSG-1

 ]]

}

PosSchedulingInfo-r16 ::= SEQUENCE {

 offsetToSI-Used-r16 ENUMERATED {true} OPTIONAL, -- Need R

 posSI-Periodicity-r16 ENUMERATED {rf8, rf16, rf32, rf64, rf128, rf256, rf512},

 posSI-BroadcastStatus-r16 ENUMERATED {broadcasting, notBroadcasting},

 posSIB-MappingInfo-r16 PosSIB-MappingInfo-r16,

 ...

}

PosSIB-MappingInfo-r16 ::= SEQUENCE (SIZE (1..maxSIB)) OF PosSIB-Type-r16

PosSIB-Type-r16 ::= SEQUENCE {

 encrypted-r16 ENUMERATED { true } OPTIONAL, -- Need R

 gnss-id-r16 GNSS-ID-r16 OPTIONAL, -- Need R

 sbas-id-r16 SBAS-ID-r16 OPTIONAL, -- Cond GNSS-ID-SBAS

 posSibType-r16 ENUMERATED { posSibType1-1, posSibType1-2, posSibType1-3, posSibType1-4, posSibType1-5, posSibType1-6,

 posSibType1-7, posSibType1-8, posSibType2-1, posSibType2-2, posSibType2-3, posSibType2-4,

 posSibType2-5, posSibType2-6, posSibType2-7, posSibType2-8, posSibType2-9, posSibType2-10,

 posSibType2-11, posSibType2-12, posSibType2-13, posSibType2-14, posSibType2-15,

 posSibType2-16, posSibType2-17, posSibType2-18, posSibType2-19, posSibType2-20,

 posSibType2-21, posSibType2-22, posSibType2-23, posSibType3-1, posSibType4-1,

 posSibType5-1,posSibType6-1, posSibType6-2, posSibType6-3,... },

 areaScope-r16 ENUMERATED {true} OPTIONAL -- Need S

}

GNSS-ID-r16 ::= SEQUENCE {

 gnss-id-r16 ENUMERATED{gps, sbas, qzss, galileo, glonass, bds, ..., navic-v1760, bds-v1770},

 ...

}

SBAS-ID-r16 ::= SEQUENCE {

 sbas-id-r16 ENUMERATED { waas, egnos, msas, gagan, ...},

 ...

}

-- TAG-POSSI-SCHEDULINGINFO-STOP

-- ASN1STOP

|  |
| --- |
| ***PosSI-SchedulingInfo* field descriptions** |
| ***gnss-id***The presence of this field indicates that the positioning SIB type is for a specific GNSS. Indicates a specific GNSS (see also TS 37.355 [49]).This field is set to *bds-v1770*, if the reference signal ofSSR correction in *posSibType2-17* is BDS B1C as specified in TS 37.355 [49]. |

There are concerns on the back compatible on the broadcast functionality. Below please find the analysis:

If only the network is implemented according to the CR and the UE is not, the B1I device won't send the request based on B1C to network, the broadcast of SSR still is based on B1I. No interoperability problems are foreseen.

If only the UE is implemented according to the CR and the network is not, there is no *bds-v1770* in the *PosSchedulingInfo* no interoperability problems are foreseen.

**Question 2**: Please provide comments below regarding the addition of the new value of GNSS ID and the description change of the affected IE.

|  |  |
| --- | --- |
| Company | Comments |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

## 3.3 Any other comments

**Question 3**: please provide any additional comment; e.g. any additional impacts foreseen

|  |  |
| --- | --- |
| Company | Comments |
|  |  |
|  |  |
|  |  |
|  |  |

**Summary:**

# 4 Conclusion

TBD